**3GPP TSG-SA WG6 Meeting #36-BIS-e S6-200570**

**E-meeting, 31st March – 8th April 2020 (revision of S6-200539)**

|  |
| --- |
| *CR-Form-v12.0* |
| **CHANGE REQUEST** |
|  |
|  | **23.379** | **CR** | **257** | **rev** | **1** | **Current version:** | **17.2.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Minor corrections of the informational elements |
|  |  |
| ***Source to WG:*** | Samsung |
| ***Source to TSG:*** | S6 |
|  |  |
| ***Work item code:*** | enh3MCPTT |  | ***Date:*** | 2020-04-07 |
|  |  |  |  |  |
| ***Category:*** | **D** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)**Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)* |
|  |  |
| ***Reason for change:*** | MCPTT Group is being used instead of MCPTT Group ID in the information element |
|  |  |
| ***Summary of change:*** | Replaced MCPTT Group with MCPTT Group ID |
|  |  |
| ***Consequences if not approved:*** | It will be misleading for stage 3 |
|  |  |
| ***Clauses affected:*** | 10.16.2.1 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

\* \* \* \* \* \* \* FIRST CHANGE \* \* \* \* \* \* \*

##### 10.16.2.1 Remotely initiated MCPTT call request

Table 10.16.2.1-1 describes the information flow remotely initiated MCPTT call request from the MCPTT client to the MCPTT server and from the MCPTT server to MCPTT client.

Table 10.16.2.1-1: remotely initiated MCPTT call request information elements

|  |  |  |
| --- | --- | --- |
| Information Element | Status | Description |
| MCPTT ID | M | The MCPTT ID of the called party (remote) |
| Notification to remote user of remotely initiated call | M | Use to determine whether the called party (remote) receives any indication of the remotely initiated MCPTT call. |
| MCPTT ID | O (NOTE) | For a remotely initiated MCPTT private call the MCPTT User ID to be called  |
| MCPTT Group ID | O (NOTE) | For a remotely initiated MCPTT group call to use. |
| NOTE: One and only one of these shall be present. |

\* \* \* \* \* \* \* END CHANGE \* \* \* \* \* \* \*