**3GPP TSG-SA WG6 Meeting #52-BIS-e S6-230246**

**e-meeting, 11th – 20th January 2023 (revision of S6-23xxxx)**

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  | **23.434** | **CR** | **0162** | **rev** | **-** | **Current version:** | **18.3.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Alignment between TS 23.434 and TS 23.436 |
|  |  |
| ***Source to WG:*** | Huawei, Hisilicon |
| ***Source to TSG:*** | S6 |
|  |  |
| ***Work item code:*** | ADAES |  | ***Date:*** | 2023-01-04 |
|  |  |  |  |  |
| ***Category:*** | **D** |  | ***Release:*** | Rel-18 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | As per the endorsement in S6-221695, the content for ADAES is to be aligned with the new TS 23.436 for Rel.18.The functional model in clause 19.2 is to be moved to TS 23.436 |
|  |  |
| ***Summary of change:*** | The functional model in clause 19.2 is moved to TS 23.436The procedures clause in 19.3 is removed. |
|  |  |
| ***Consequences if not approved:*** | The alignment as per the endorsement in S6-221695 will not be achieved. |
|  |  |
| ***Clauses affected:*** | 19, 19.1, 19.2 and its subclauses, 19.3. |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

\* \* \* First Change \* \* \* \*

# 19 Application Data Analytics Enablement

## 19.1 General

The application data analytics enablement is a SEAL service that offers value-add application data analytics capabilities which cover stats/predictions for the end-to-end application service. Considering vertical-specific applications and edge applications as the major consumers of 3GPP-provided data analytics services, the application enablement layer can play role on the exposure of data analytics services from different 3GPP domains to the vertical/ASP in a unified manner; and on defining, at an overarching layer, value-add application data analytics services which cover stats/predictions for the end-to-end application service. The detailed specification of ADAE is provided in 3GPP TS 23.436 [49].