- No.: 2
- Timestamp: 17:16:42:326_0
- RFN: 102
- Chip: 30464
- Event: Start Timer
- Source: tc_12_4_1_4c2 LINE 1
- Message Structure:
no details available
- Constraint:
t_Guard (900 Sec)
- BinaryMessage:

- No.: 60
- Timestamp: 17:16:42:334_0
- RFN: 103
- Chip: 23040
- Event: Send
- PCO: Ut
- Message: MMI_CmdReq
- Source: ts_MMI_SetOpModeA LINE 1
- Message Structure:
MMI_CmdReq < Exp>
. (IA5StringType)cmd = -1 <"Please set UE in operation mode A (to support simulataneous CS and PS services>
- Constraint:
ca_MMI_CmdReq
- BinaryMessage:
50 6c 65 61 73 65 20 73 65 74 20 55 45 20 69 6e 20 6f 70 65 72 61 74 69 6f 6e 20 6d 6f 64 65 20 41 20 28 74 6f 20 73 75 70 70 6f 72 74 20 73 69 6d 75 6c 61 74 61 6e 65 6f 75 73 20 43 53 20 61 6e 64 20 50 53 20 73 65 72 76 69 63 65 73 29 20

- No.: 64
- Timestamp: 17:16:42:507_0
- RFN: 120
- Chip: 33792
- Event: Receive
- PCO: Ut
- Message: MMI_CmdCnf
- Source: ts_MMI_SetOpModeA LINE 2
- Message Structure:
MMI_CmdCnf
. (BooleanType)result = TRUE
. (IA5StringType)resultString[6] = " OK "
- Constraint:
ca_MMI_CmdCnf
- BinaryMessage:
80 0d 0a 4f 4b 0d 0a

- No.: 108
- Timestamp: 17:16:42:513_0
- RFN: 121
- Chip: 16896
- Event: Send
- PCO: Ut
- Message: MMI_CmdReq
- Source: ts_MMI_UE_SwitchOff LINE 2
- Message Structure:
MMI_CmdReq
. (IA5StringType)cmd[-1] = "Please switch off the UE"
- Constraint:
ca_MMI_CmdReq
- BinaryMessage:
50 6c 65 61 73 65 20 73 77 69 74 63 68 20 6f 66 66 20 20 74 68 65 20 55 45

- No.: 112
- Timestamp: 17:16:46:654_0
- RFN: 535
- Chip: 24832
- Event: Receive
- PCO: Ut
- Message: MMI_CmdCnf
- Source: ts_MMI_UE_SwitchOff LINE 3
- Message Structure:
MMI_CmdCnf
. (BooleanType)result = TRUE
. (IA5StringType)resultString[6] = " OK "
- Constraint:
ca_MMI_CmdCnf
- BinaryMessage:
80 0d 0a 4f 4b 0d 0a

- No.: 117
- Timestamp: 17:16:46:655_4
- RFN: 535
- Chip: 28672
- Event: Send
- PCO: CPHY
- Message: CPHY_Ini_REQ
- Source: ts_SS_CellCfg:lt_CelllsAlreadyStarted LINE 5
- Message Structure:
CPHY_Ini_REQ
. (CPHY_Ini_REQ)CPHY_Ini_REQ[-1] = 0
- Constraint:
cas_InitReqDef
- BinaryMessage:
0a 01 00

- No.: 118
- Timestamp: 17:16:46:656_0
- RFN: 535
- Chip: 30208
- Event: Receive
- PCO: CPHY
- Message: CPHY_Ini_CNF
- Source: ts_SS_CellCfg:lt_CelllsAlreadyStarted LINE 6
- Message Structure:
CPHY_Ini_CNF
- Constraint:
car_IniCnf
- BinaryMessage:
30 02 05 00

- No.: 122
- Timestamp: 17:16:46:657_0
- RFN: 535
- Chip: 35072
- Event: Send
- PCO: CPHY
- Message: CPHY_Cell_Config_REQ
- Source: ts_SS_CellCfg LINE 6
- Message Structure:
CPHY_Cell_Config_REQ
. (IntegerType)cellId[-1] = 0
. (IntegerType)tcell[-1] = 0
. (IntegerType)sfnOffset[-1] = 0
. FrequencyInfo
. . modeSpecificInfo
. . . FrequencyInfoFDD
. . . . (IntegerType)uarfcn_UL[-1] = -
. . . . (IntegerType)uarfcn_DL[-1] = 10700
. (IntegerType)primaryScramblingCode_SS[-1] = 100
. CellTxPowerLevel
. (IntegerType)dLTxAttenuationLevel[-1] = 0
- Constraint:
ca_CellCfgReq
- BinaryMessage:
30 19 02 01 00 02 01 00 02 01 00 30 06 30 04 02 02 29 cc 02 01 64 05 00 02 01 00

- No.: 129
- Timestamp: 17:16:46:733_0
- RFN: 543
- Chip: 20992
- Event: Receive
- PCO: CPHY
- Message: CPHY_Cell_Config_CNF
- Source: ts_SS_CellCfg LINE 7
- Message Structure:
CPHY_Cell_Config_CNF
. (IntegerType)cellId[0] = 0
- Constraint:
ca_CellCfgCnf
- BinaryMessage:
30 03 02 01 00

- No.: 141
- Timestamp: 17:16:46:735_0
- RFN: 543
- Chip: 29696
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 3
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 0
. (RatType)ratType[0] = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . PrimaryCPICHInfo
. . . . (IntegerType)dl_TxPower_PCPICH[-1] = -60
. . . . (BooleanType)txdiversityIndicator = FALSE
- Constraint:
ca_pCPICH_Info
- BinaryMessage:
30 13 02 01 00 02 01 00 0a 01 00 30 08 30 06 02 01 c4 01 01 00

- No.: 145
- Timestamp: 17:16:46:741_0
- RFN: 544
- Chip: 12800
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 4
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 0
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 00

- No.: 146
- Timestamp: 17:16:46:742_0
- RFN: 544
- Chip: 16896
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 5
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 1
. (RatType)ratType[0] = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . PrimarySCHInfo
. . . . (BooleanType)tstdIndicator = FALSE
. . . . (IntegerType)dl_TxPower[-1] = -5
- Constraint:
ca_pSCH_Info
- BinaryMessage:
30 13 02 01 00 02 01 01 0a 01 00 30 08 30 06 01 01 00 02 01 fb

- No.: 150
- Timestamp: 17:16:46:746_0
- RFN: 544
- Chip: 32000
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 6
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 1
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 01

- No.: 151
- Timestamp: 17:16:46:747_0
- RFN: 544
- Chip: 36352
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 7
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 2
. (RatType)ratType[0] = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . SecondarySCHInfo
. . . . (BooleanType)tstdIndicator = FALSE
. . . . (IntegerType)dl_TxPower[-1] = -5
- Constraint:
ca_sSCH_Info
- BinaryMessage:
30 13 02 01 00 02 01 02 0a 01 00 30 08 30 06 01 01 00 02 01 fb

- No.: 155
- Timestamp: 17:16:46:886_0
- RFN: 558
- Chip: 31488
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 8
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 2
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 02

- No.: 156
- Timestamp: 17:16:46:887_0
- RFN: 558
- Chip: 35072
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 9
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 4
. (RatType)ratType[0] = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . PrimaryCCPCHInfo
. . . . (BooleanType)sttd_Indicator = FALSE
. . . . (IntegerType)dl_TxPower[-1] = -2
- Constraint:
ca_pCCPCH_Info
- BinaryMessage:
30 13 02 01 00 02 01 04 0a 01 00 30 08 30 06 01 01 00 02 01 fe

- No.: 160
- Timestamp: 17:16:46:895_0
- RFN: 559
- Chip: 24832
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 10
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 4
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 04

- No.: 161
- Timestamp: 17:16:46:898_0
- RFN: 560
- Chip: 512
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Config_REQ
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 11
- Message Structure:
CPHY_TrCH_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 4
. (RatType)ratType[0] = 0
. TrChConfigType
. CphyTrchConfigReq
. . SS_ActivationTime
. . ulconnectedTrCHList
. . TFCS
. . dlconnectedTrCHList
. . . CphyTrchConfigReq_setseq_1
. . . . (IntegerType)trchid[-1] = 11
. . . . (SS_DL_TransportChannelType)dl_TransportChannelType[0] = 2
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size[-1] = 246
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional[0] = 0
. . . . . . (IntegerType)rateMatchingAttribute[-1] = 1
. . . . . . (CRC_Size)crc_Size[0] = 3
. . TFCS
. . . ExplicitTFCS_Configuration
. . . . TFCS_ReconfAdd
. . . . . ctfcSize
. . . . . . ctfc2Bit
. . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . (IntegerType)ctfc2[-1] = 0
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . fdd
. . . . . . . . . . . . . (IntegerType)gainFactorBetaC[-1] = 11
. . . . . . . . . . . (IntegerType)gainFactorBetaD[-1] = 15
. . . . . . . . . . . (IntegerType)referenceTFC_ID[-1] = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
- Constraint:
ca_BCH_InfoActNow
- BinaryMessage:
30 4c 02 01 00 02 01 04 0a 01 00 05 00 30 3f 05 00 30 23 30 21 02 01 0b 0a 01 02 30 19 30 0c 30 0a 02 02 00 f6 30 02 05 00 05 00 30 09 0a 01 00 02 01 01 0a 01 03 30 16 30 14 30 12 02 01 00 30 0d 30 0b 30 03 02 01 0b 02 01 0f 02 01 00

- No.: 165
- Timestamp: 17:16:46:906_0
- RFN: 560
- Chip: 29184
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Config_CNF
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 12
- Message Structure:
CPHY_TrCH_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 4
- Constraint:
ca_TrChCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 04

- No.: 166
- Timestamp: 17:16:46:911_0
- RFN: 561
- Chip: 11008
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 13
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 4
. (RatType)ratType[0] = 0
. configMessage
. . CmacConfigReq
. . . SS_ActivationTime
. . . UE_Info
. . . . U_RNTI
. . . . (BitStringType)c_RNTI[16] = -
. . . TrCHInfo
. . . . ulconnectedTrCHList
. . . . TFCS
. . . . dlconnectedTrCHList
. . . . . TrCHInfo_setseq_1
. . . . . . (IntegerType)trchid[-1] = 11
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size[-1] = 246
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional[0] = 0
. . . . . . . . (IntegerType)rateMatchingAttribute[-1] = 1
. . . . . . . . (CRC_Size)crc_Size[0] = 3
. . . . TFCS
. . . . . ExplicitTFCS_Configuration
. . . . . . TFCS_ReconfAdd
. . . . . . . ctfcSize
. . . . . . . . ctfc2Bit
. . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . (IntegerType)ctfc2[-1] = 0
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC[-1] = 11
. . . . . . . . . . . . . (IntegerType)gainFactorBetaD[-1] = 15
. . . . . . . . . . . . . (IntegerType)referenceTFC_ID[-1] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . TrCH_LogCHMappingList1
. . . . ulconnectedTrCHList
. . . . dlconnectedTrCHList
. . . . . TrCH_LogCHMappingList1_setseq_1
. . . . . . (IntegerType)trchid[-1] = 11
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation[0] = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType[0] = 2
. . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . . . (LogicalChannelType)logicalChannelType[0] = 0
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 1
. . . . . . . . (IntegerType)rB_Identity[-1] = -1
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_CMAC_CfgInfo
- BinaryMessage:
30 6e 02 01 00 02 01 04 0a 01 00 30 63 05 00 30 00 30 3a 30 20 30 1e 02 01 0b 30 19 30 0c 30 0a 02 02 00 f6 30 02 05 00 05 00 30 09 0a 01 00 02 01 01 0a 01 03 30 16 30 14 30 12 02 01 00 30 0d 30 0b 30 03 02 01 0b 02 01 0f 02 01 00 30 21 30 1f 30 1d 02 01 0b 30 18 30 16 30 11 0a 01 00 0a 01 02 02 01 01 0a 01 00 05 00 02 01 01 02 01 ff

- No.: 170
- Timestamp: 17:16:46:914_0
- RFN: 561
- Chip: 23040
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 14
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 4
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 04

- No.: 178
- Timestamp: 17:16:46:916_0
- RFN: 561
- Chip: 29952
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_PCH_FACH_CCCH_Cfg LINE 3
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 5
. (RatType)ratType[0] = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . SecondaryCCPCHInfo
. . . . (IntegerType)scramblingCode[-1] = 0
. . . . SF256_AndCodeNumber
. . . . . (IntegerType)sf64[-1] = 1
. . . . (IntegerType)sCCPCHSlotFormat[-1] = 8
. . . . (IntegerType)timingOffset[-1] = 0
. . . . (PositionFixedOrFlexible)positionFixedOrFlexible[0] = 1
. . . . (BooleanType)sttd_Indicator = FALSE
. . . . (IntegerType)dl_TxPower[-1] = -2
. . . . (IntegerType)powerOffsetOfTFCI_PO1[-1] = 6
. . . . (IntegerType)powerOffsetOfPILOT_PO3[-1] = 6
- Constraint:
ca_sCCPCH_Info
- BinaryMessage:
30 28 02 01 00 02 01 05 0a 01 00 30 1d 30 1b 02 01 00 02 01 01 02 01 08 02 01 00 0a 01 01 01 01 00 02 01 fe 02 01 06 02 01 06

- No.: 182
- Timestamp: 17:16:46:922_0
- RFN: 562
- Chip: 14336
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_PCH_FACH_CCCH_Cfg LINE 4
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 5
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 05

- No.: 183
- Timestamp: 17:16:46:929_0
- RFN: 563
- Chip: 3840
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Config_REQ
- Source: ts_SS_PCH_FACH_CCCH_Cfg LINE 5
- Message Structure:
CPHY_TrCH_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 5
. (RatType)ratType[0] = 0
. TrChConfigType
. CphyTrchConfigReq
. . SS_ActivationTime
. . ulconnectedTrCHList
. . TFCS
. . dlconnectedTrCHList
. . . CphyTrchConfigReq_setseq_1
. . . . (IntegerType)trchid[-1] = 12
. . . . (SS_DL_TransportChannelType)dl_TransportChannelType[0] = 3
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size[-1] = 240
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional[0] = 0
. . . . . . (IntegerType)rateMatchingAttribute[-1] = 230
. . . . . . (CRC_Size)crc_Size[0] = 3
. . . CphyTrchConfigReq_setseq_1
. . . . (IntegerType)trchid[-1] = 13
. . . . (SS_DL_TransportChannelType)dl_TransportChannelType[0] = 1
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size[-1] = 168
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . (IntegerType)small[-1] = 2
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional[0] = 0
. . . . . . (IntegerType)rateMatchingAttribute[-1] = 220
. . . . . . (CRC_Size)crc_Size[0] = 3
. . . CphyTrchConfigReq_setseq_1
. . . . (IntegerType)trchid[-1] = 14
. . . . (SS_DL_TransportChannelType)dl_TransportChannelType[0] = 1
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size[-1] = 360
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . (IntegerType)rateMatchingAttribute[-1] = 130
. . . . . . (CRC_Size)crc_Size[0] = 3
. . TFCS
. . . ExplicitTFCS_Configuration
. . . . TFCS_ReconfAdd
. . . . . ctfcSize
. . . . . . ctfc4Bit
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4[-1] = 0
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4[-1] = 1
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4[-1] = 2
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4[-1] = 3
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4[-1] = 4
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4[-1] = 5
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4[-1] = 6
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4[-1] = 8
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . fdd
. . . . . . . . . . . . . (IntegerType)gainFactorBetaC[-1] = 11
. . . . . . . . . . . (IntegerType)gainFactorBetaD[-1] = 15
. . . . . . . . . . . (IntegerType)referenceTFC_ID[-1] = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
- Constraint:
ca_PCH_2_FACH_InfoActNow
- BinaryMessage:
30 81 e4 02 01 00 02 01 05 0a 01 00 05 00 30 81 d6 05 00 30 74 30 24 02 01 0c 0a 01 03 30 1c 30 0e 30 0c 02 02 00 f0 30 04 05 00 05 00 05 00 30 0a 0a 01 00 02 02 00 e6 0a 01 03 30 27 02 01 0d 0a 01 01 30 1f 30 11 30 0f 02 02 00 a8 30 07 05 00 05 00 02 01 02 05 00 30 0a 0a 01 00 02 02 00 dc 0a 01 03 30 23 02 01 0e 0a 01 01 30 1b 30 0e 30 0c 02 02 01 68 30 04 05 00 05 00 05 00 30 09 05 00 02 02 00 82 0a 01 03 30 5c 30 5a 30 08 02 01 00 30 03 02 01 00 30 08 02 01 01 30 03 02 01 00 30 08 02 01 02 30 03 02 01 00 30 08 02 01 03 30 03 02 01 00 30 08 02 01 04 30 03 02 01 00 30 08 02 01 05 30 03 02 01 00 30 08 02 01 06 30 03 02 01 00 30 12 02 01 08 30 0d 30 0b 30 03 02 01 0b 02 01 0f 02 01 00

- No.: 187
- Timestamp: 17:16:46:942_0
- RFN: 564
- Chip: 14336
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Config_CNF
- Source: ts_SS_PCH_FACH_CCCH_Cfg LINE 6
- Message Structure:
CPHY_TrCH_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 5
- Constraint:
ca_TrChCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 05

- No.: 188
- Timestamp: 17:16:46:952_0
- RFN: 565
- Chip: 15616
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_SS_PCH_FACH_CCCH_Cfg LINE 7
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 5
. (RatType)ratType[0] = 0
. configMessage
. . CmacConfigReq
. . . SS_ActivationTime
. . . UE_Info
. . . . U_RNTI
. . . . (BitStringType)c_RNTI[16] = -
. . . TrCHInfo
. . . . ulconnectedTrCHList
. . . . TFCS
. . . . dlconnectedTrCHList
. . . . . TrCHInfo_setseq_1
. . . . . . (IntegerType)trchid[-1] = 12
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size[-1] = 240
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional[0] = 0
. . . . . . . . (IntegerType)rateMatchingAttribute[-1] = 230
. . . . . . . . (CRC_Size)crc_Size[0] = 3
. . . . . TrCHInfo_setseq_1
. . . . . . (IntegerType)trchid[-1] = 13
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size[-1] = 168
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . (IntegerType)small[-1] = 2
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional[0] = 0
. . . . . . . . (IntegerType)rateMatchingAttribute[-1] = 220
. . . . . . . . (CRC_Size)crc_Size[0] = 3
. . . . . TrCHInfo_setseq_1
. . . . . . (IntegerType)trchid[-1] = 14
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size[-1] = 360
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . (IntegerType)rateMatchingAttribute[-1] = 130
. . . . . . . . (CRC_Size)crc_Size[0] = 3
. . . . TFCS
. . . . . ExplicitTFCS_Configuration
. . . . . . TFCS_ReconfAdd
. . . . . . . ctfcSize
. . . . . . . . ctfc4Bit
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4[-1] = 0
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4[-1] = 1
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4[-1] = 2
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4[-1] = 3
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4[-1] = 4
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4[-1] = 5
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4[-1] = 6
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4[-1] = 8
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC[-1] = 11
. . . . . . . . . . . . . (IntegerType)gainFactorBetaD[-1] = 15
. . . . . . . . . . . . . (IntegerType)referenceTFC_ID[-1] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . TrCH_LogCHMappingList1
. . . . ulconnectedTrCHList
. . . . dlconnectedTrCHList
. . . . . TrCH_LogCHMappingList1_setseq_1
. . . . . . (IntegerType)trchid[-1] = 12
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation[0] = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType[0] = 3
. . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . . . (LogicalChannelType)logicalChannelType[0] = 1
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 1
. . . . . . . . (IntegerType)rB_Identity[-1] = -2
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
. . . . . TrCH_LogCHMappingList1_setseq_1
. . . . . . (IntegerType)trchid[-1] = 13
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation[0] = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType[0] = 1
. . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 5
. . . . . . . . . . (LogicalChannelType)logicalChannelType[0] = 2
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 1
. . . . . . . . (IntegerType)rB_Identity[-1] = 0
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_CMAC_CfgInfo
- BinaryMessage:
30 82 01 21 02 01 00 02 01 05 0a 01 00 30 82 01 14 05 00 30 00 30 81 cb 30 6b 30 21 02 01 0c 30 1c 30 0e 30 0c 02 02 00 f0 30 04 05 00 05 00 05 00 30 0a 0a 01 00 02 02 00 e6 0a 01 03 30 24 02 01 0d 30 1f 30 11 30 0f 02 02 00 a8 30 07 05 00 05 00 02 01 02 05 00 30 0a 0a 01 00 02 02 00 dc 0a 01 03 30 20 02 01 0e 30 1b 30 0e 30 0c 02 02 01 68 30 04 05 00 05 00 05 00 30 09 05 00 02 02 00 82 0a 01 03 30 5c 30 5a 30 08 02 01 00 30 03 02 01 00 30 08 02 01 01 30 03 02 01 00 30 08 02 01 02 30 03 02 01 00 30 08 02 01 03 30 03 02 01 00 30 08 02 01 04 30 03 02 01 00 30 08 02 01 05 30 03 02 01 00 30 08 02 01 06 30 03 02 01 00 30 12 02 01 08 30 0d 30 0b 30 03 02 01 0b 02 01 0f 02 01 00 30 40 30 3e 30 1d 02 01 0c 30 18 30 16 30 11 0a 01 00 0a 01 03 02 01 01 0a 01 01 05 00 02 01 01 02 01 fe 30 1d 02 01 0d 30 18 30 16 30 11 0a 01 00 0a 01 01 02 01 05 0a 01 02 05 00 02 01 01 02 01 00

- No.: 192
- Timestamp: 17:16:46:958_0
- RFN: 566
- Chip: 256
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_SS_PCH_FACH_CCCH_Cfg LINE 8
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 5
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 05

- No.: 193
- Timestamp: 17:16:46:959_0
- RFN: 566
- Chip: 4864
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_PCH_FACH_CCCH_Cfg LINE 9
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 6
. (RatType)ratType[0] = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . PICHInfo
. . . . PICH_Info
. . . . . fdd
. . . . . . (IntegerType)channelisationCode256[-1] = 2
. . . . . . (PI_CountPerFrame)pi_CountPerFrame[0] = 0
. . . . . . (BooleanType)sttd_Indicator = FALSE
. . . . (IntegerType)dl_TxPower[-1] = -5
. . . . (IntegerType)sccpchId_associated[-1] = 5
- Constraint:
ca_PICH_Info
- BinaryMessage:
30 1e 02 01 00 02 01 06 0a 01 00 30 13 30 11 30 09 02 01 02 0a 01 00 01 01 00 02 01 fb 02 01 05

- No.: 197
- Timestamp: 17:16:46:965_0
- RFN: 566
- Chip: 25600
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_PCH_FACH_CCCH_Cfg LINE 10
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 6
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 06

- No.: 205
- Timestamp: 17:16:46:966_1
- RFN: 566
- Chip: 32000
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_RACH_CCCH_Cfg LINE 3
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 7
. (RatType)ratType[0] = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . AICHInfo
. . . . AICH_Info
. . . . . (IntegerType)channelisationCode256[-1] = 3
. . . . . (BooleanType)sttd_Indicator = FALSE
. . . . . (AICH_TransmissionTiming)aich_TransmissionTiming[0] = 0
. . . . (IntegerType)dl_TxPower[-1] = -5
- Constraint:
ca_AichInfo
- BinaryMessage:
30 1b 02 01 00 02 01 07 0a 01 00 30 10 30 0e 30 09 02 01 03 01 01 00 0a 01 00 02 01 fb

- No.: 209
- Timestamp: 17:16:46:973_0
- RFN: 567
- Chip: 18688
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_RACH_CCCH_Cfg LINE 4
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 7
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 07

- No.: 210
- Timestamp: 17:16:46:974_0
- RFN: 567
- Chip: 22272
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_RACH_CCCH_Cfg LINE 5
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 8
. (RatType)ratType[0] = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . PRACHInfo
. . . . fdd_tdd
. . . . . fdd
. . . . . . (BitStringType)preambleSignature[16] = "0000000011111111"
. . . . . . (SF_PRACH)spreadingFactorForDataPart[0] = 1
. . . . . . (IntegerType)preambleScramblingCode[-1] = 0
. . . . . . (PuncturingLimit)puncturingLimit[0] = 15
. . . . . . (BitStringType)accessSlot[12] = "111111111111"
- Constraint:
ca_PRACH_Info
- BinaryMessage:
30 22 02 01 00 02 01 08 0a 01 00 30 17 30 15 30 13 03 03 00 00 ff 0a 01 01 02 01 00 0a 01 0f 03 03 04 ff f0

- No.: 214
- Timestamp: 17:16:46:978_0
- RFN: 568
- Chip: 2048
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_RACH_CCCH_Cfg LINE 6
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 8
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 08

- No.: 215
- Timestamp: 17:16:46:981_0
- RFN: 568
- Chip: 12032
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Config_REQ
- Source: ts_SS_RACH_CCCH_Cfg LINE 7
- Message Structure:
CPHY_TrCH_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 8
. (RatType)ratType[0] = 0
. TrChConfigType
. CphyTrchConfigReq
. . SS_ActivationTime
. . ulconnectedTrCHList
. . . CphyTrchConfigReq_setseq_0
. . . . (IntegerType)trchid[-1] = 15
. . . . (SS_UL_TransportChannelType)ul_TransportChannelType[0] = 1
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size[-1] = 168
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size[-1] = 360
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional[0] = 0
. . . . . . (IntegerType)rateMatchingAttribute[-1] = 150
. . . . . . (CRC_Size)crc_Size[0] = 3
. . TFCS
. . . ExplicitTFCS_Configuration
. . . . TFCS_ReconfAdd
. . . . . ctfcSize
. . . . . . ctfc2Bit
. . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . (IntegerType)ctfc2[-1] = 0
. . . . . . . . PowerOffsetInformation
. . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . (IntegerType)ctfc2[-1] = 1
. . . . . . . . PowerOffsetInformation
. . dlconnectedTrCHList
. . TFCS
- Constraint:
cab_RACH_InfoActNow
- BinaryMessage:
30 4f 02 01 00 02 01 08 0a 01 00 05 00 30 42 05 00 30 30 30 2e 02 01 0f 0a 01 01 30 26 30 18 30 0a 02 02 00 a8 30 02 05 00 05 00 30 0a 02 02 01 68 30 02 05 00 05 00 30 0a 0a 01 00 02 02 00 96 0a 01 03 30 0c 30 0a 30 03 02 01 00 30 03 02 01 01

- No.: 219
- Timestamp: 17:16:46:992_0
- RFN: 569
- Chip: 17152
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Config_CNF
- Source: ts_SS_RACH_CCCH_Cfg LINE 8
- Message Structure:
CPHY_TrCH_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 8
- Constraint:
ca_TrChCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 08

- No.: 220
- Timestamp: 17:16:46:996_0
- RFN: 569
- Chip: 33024
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_SS_RACH_CCCH_Cfg LINE 9
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 8
. (RatType)ratType[0] = 0
. configMessage
. . CmacConfigReq
. . . SS_ActivationTime
. . . UE_Info
. . . . U_RNTI
. . . . (BitStringType)c_RNTI[16] = -
. . . TrCHInfo
. . . . ulconnectedTrCHList
. . . . . TrCHInfo_setseq_0
. . . . . . (IntegerType)trchid[-1] = 15
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size[-1] = 168
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size[-1] = 360
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional[0] = 0
. . . . . . . . (IntegerType)rateMatchingAttribute[-1] = 150
. . . . . . . . (CRC_Size)crc_Size[0] = 3
. . . . TFCS
. . . . . ExplicitTFCS_Configuration
. . . . . . TFCS_ReconfAdd
. . . . . . . ctfcSize
. . . . . . . . ctfc2Bit
. . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . (IntegerType)ctfc2[-1] = 0
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . (IntegerType)ctfc2[-1] = 1
. . . . . . . . . . PowerOffsetInformation
. . . . dlconnectedTrCHList
. . . . TFCS
. . . TrCH_LogCHMappingList1
. . . . ulconnectedTrCHList
. . . . . TrCH_LogCHMappingList1_setseq_0
. . . . . . (IntegerType)trchid[-1] = 15
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation[0] = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType[0] = 1
. . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 5
. . . . . . . . . . (LogicalChannelType)logicalChannelType[0] = 2
. . . . . . . . (IntegerType)rB_Identity[-1] = 0
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
. . . . dlconnectedTrCHList
- Constraint:
ca_CMAC_CfgInfo
- BinaryMessage:
30 6c 02 01 00 02 01 08 0a 01 00 30 61 05 00 30 00 30 3d 30 2d 30 2b 02 01 0f 30 26 30 18 30 0a 02 02 00 a8 30 02 05 00 05 00 30 0a 02 02 01 68 30 02 05 00 05 00 30 0a 0a 01 00 02 02 00 96 0a 01 03 30 0c 30 0a 30 03 02 01 00 30 03 02 01 01 30 1c 30 1a 30 18 02 01 0f 30 13 30 11 30 0c 0a 01 00 0a 01 01 02 01 05 0a 01 02 02 01 00

- No.: 224
- Timestamp: 17:16:47:002_0
- RFN: 570
- Chip: 16384
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_SS_RACH_CCCH_Cfg LINE 10
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 8
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 08

- No.: 261
- Timestamp: 17:16:47:009_0
- RFN: 571
- Chip: 5120
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_1DCH_DCCH_Cfg LINE 4
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 26
. (RatType)ratType[0] = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . DPCHInfo
. . . . UL_DPCH_Info
. . . . DL_DPCHInfo
. . . . . DL_CommonInformation
. . . . . . DL_DPCH_InfoCommon
. . . . . . . cfnHandling
. . . . . . . . initialise
. . . . . . . . . (IntegerType)cfntargetsfnframeoffset[-1] = -
. . . . . . . modeSpecificInfo
. . . . . . . . fdd
. . . . . . . . . DL_DPCH_PowerControlInfo
. . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . fdd
. . . . . . . . . . . . (DPC_Mode)dpc_Mode[0] = 0
. . . . . . . . . (IntegerType)powerOffsetPilot_pdpdch[-1] = 0
. . . . . . . . . Dl_rate_matching_restriction
. . . . . . . . . SF512_AndPilot
. . . . . . . . . . (PilotBits128)sfd128[0] = 0
. . . . . . . . . (PositionFixedOrFlexible)positionFixedOrFlexible[0] = 0
. . . . . . . . . (BooleanType)tfci_Existence = FALSE
. . . . . . modeSpecificInfo
. . . . . . . fdd
. . . . . . . . (IntegerType)defaultDPCH_OffsetValue[-1] = 459
. . . . . . . . DPCH_CompressedModeInfo
. . . . . . . . (TX_DiversityMode)tx_DiversityMode[0] = 0
. . . . . . . . SSDT_Information
. . . . . DL_DPCH_InfoPerRL
. . . . . . fdd
. . . . . . . (PCPICH_UsageForChannelEst)pCPICH_UsageForChannelEst[0] = 0
. . . . . . . (IntegerType)dpch_FrameOffset[-1] = 18
. . . . . . . SecondaryCPICH_Info
. . . . . . . DL_ChannelisationCodeList
. . . . . . . . DL_ChannelisationCode
. . . . . . . . . (IntegerType)secondaryScramblingCode[-1] = 1
. . . . . . . . . SF512_AndCodeNumber
. . . . . . . . . . (IntegerType)sf128[-1] = 0
. . . . . . . . . (ScramblingCodeChange)scramblingCodeChange[0] = -
. . . . . . . (IntegerType)tpc_CombinationIndex[-1] = 0
. . . . . . . (SSDT_CellIdentity)ssdt_CellIdentity[0] = -
. . . . . . . (ClosedLoopTimingAdjMode)closedLoopTimingAdjMode[0] = -
. . . . . (IntegerType)powerOffsetOfTFCI_PO1[-1] = 0
. . . . . (IntegerType)powerOffsetOfTPC_PO2[-1] = 0
. . . . . (IntegerType)powerOffsetOfPILOT_PO3[-1] = 0
. . . . . (IntegerType)dl_TxPower[-1] = -5
. . . . . (IntegerType)dl_TxPowerMax[-1] = 15
. . . . . (IntegerType)dl_TxPowerMin[-1] = -35
- Constraint:
ca_DL_DPCH_Info
- BinaryMessage:
30 5a 02 01 00 02 01 1a 0a 01 00 30 4f 30 4d 30 4b 30 22 30 17 30 00 30 13 30 05 30 03 0a 01 00 02 01 00 0a 01 00 0a 01 00 01 01 00 30 07 02 02 01 cb 0a 01 00 30 13 0a 01 00 02 01 12 30 08 30 06 02 01 01 02 01 00 02 01 00 02 01 00 02 01 00 02 01 00 02 01 fb 02 01 0f 02 01 dd

- No.: 265
- Timestamp: 17:16:47:017_0
- RFN: 571
- Chip: 33792
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_1DCH_DCCH_Cfg LINE 5
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 26
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 1a

- No.: 266
- Timestamp: 17:16:47:020_0
- RFN: 572
- Chip: 9216
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Config_REQ
- Source: ts_SS_1DCH_DCCH_Cfg LINE 6
- Message Structure:
CPHY_TrCH_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 26
. (RatType)ratType[0] = 0
. TrChConfigType
. . (TrChConfigType_list_0)dch[0] = 0
. CphyTrchConfigReq
. . SS_ActivationTime
. . ulconnectedTrCHList
. . TFCS
. . dlconnectedTrCHList
. . . CphyTrchConfigReq_setseq_1
. . . . (IntegerType)trchid[-1] = 10
. . . . (SS_DL_TransportChannelType)dl_TransportChannelType[0] = 0
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size[-1] = 148
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional[0] = 1
. . . . . . (IntegerType)rateMatchingAttribute[-1] = 192
. . . . . . (CRC_Size)crc_Size[0] = 3
. . TFCS
. . . ExplicitTFCS_Configuration
. . . . TFCS_ReconfAdd
. . . . . ctfcSize
. . . . . . ctfc2Bit
. . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . (IntegerType)ctfc2[-1] = 0
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . (IntegerType)ctfc2[-1] = 1
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . fdd
. . . . . . . . . . . . . (IntegerType)gainFactorBetaC[-1] = 11
. . . . . . . . . . . (IntegerType)gainFactorBetaD[-1] = 15
. . . . . . . . . . . (IntegerType)referenceTFC_ID[-1] = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
- Constraint:
ca_DCH_148_TTI_10_DL_InfoActNow
- BinaryMessage:
30 5a 02 01 00 02 01 1a 0a 01 00 0a 01 00 30 4c 05 00 30 26 30 24 02 01 0a 0a 01 00 30 1c 30 0e 30 0c 02 02 00 94 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 c0 0a 01 03 30 20 30 1e 30 08 02 01 00 30 03 02 01 00 30 12 02 01 01 30 0d 30 0b 30 03 02 01 0b 02 01 0f 02 01 00

- No.: 270
- Timestamp: 17:16:47:026_0
- RFN: 572
- Chip: 33280
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Config_CNF
- Source: ts_SS_1DCH_DCCH_Cfg LINE 7
- Message Structure:
CPHY_TrCH_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 26
- Constraint:
ca_TrChCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 1a

- No.: 271
- Timestamp: 17:16:47:034_0
- RFN: 573
- Chip: 25088
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_SS_1DCH_DCCH_Cfg LINE 8
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 26
. (RatType)ratType[0] = 0
. configMessage
. . CmacConfigReq
. . . SS_ActivationTime
. . . UE_Info
. . . . U_RNTI
. . . . (BitStringType)c_RNTI[16] = -
. . . TrCHInfo
. . . . ulconnectedTrCHList
. . . . TFCS
. . . . dlconnectedTrCHList
. . . . . TrCHInfo_setseq_1
. . . . . . (IntegerType)trchid[-1] = 10
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size[-1] = 148
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional[0] = 1
. . . . . . . . (IntegerType)rateMatchingAttribute[-1] = 192
. . . . . . . . (CRC_Size)crc_Size[0] = 3
. . . . TFCS
. . . . . ExplicitTFCS_Configuration
. . . . . . TFCS_ReconfAdd
. . . . . . . ctfcSize
. . . . . . . . ctfc2Bit
. . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . (IntegerType)ctfc2[-1] = 0
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . (IntegerType)ctfc2[-1] = 1
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC[-1] = 11
. . . . . . . . . . . . . (IntegerType)gainFactorBetaD[-1] = 15
. . . . . . . . . . . . . (IntegerType)referenceTFC_ID[-1] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . TrCH_LogCHMappingList1
. . . . ulconnectedTrCHList
. . . . dlconnectedTrCHList
. . . . . TrCH_LogCHMappingList1_setseq_1
. . . . . . (IntegerType)trchid[-1] = 10
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation[0] = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType[0] = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . . . (LogicalChannelType)logicalChannelType[0] = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 1
. . . . . . . . (IntegerType)rB_Identity[-1] = 1
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation[0] = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType[0] = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 2
. . . . . . . . . . (LogicalChannelType)logicalChannelType[0] = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 2
. . . . . . . . (IntegerType)rB_Identity[-1] = 2
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation[0] = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType[0] = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 3
. . . . . . . . . . (LogicalChannelType)logicalChannelType[0] = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 3
. . . . . . . . (IntegerType)rB_Identity[-1] = 3
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation[0] = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType[0] = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 4
. . . . . . . . . . (LogicalChannelType)logicalChannelType[0] = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 4
. . . . . . . . (IntegerType)rB_Identity[-1] = 4
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_CMAC_CfgInfo
- BinaryMessage:
30 81 c4 02 01 ff 02 01 1a 0a 01 00 30 81 b8 05 00 30 00 30 47 30 23 30 21 02 01 0a 30 1c 30 0e 30 0c 02 02 00 94 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 c0 0a 01 03 30 20 30 1e 30 08 02 01 00 30 03 02 01 00 30 12 02 01 01 30 0d 30 0b 30 03 02 01 0b 02 01 0f 02 01 00 30 69 30 67 30 65 02 01 0a 30 60 30 16 30 11 0a 01 00 0a 01 00 02 01 01 0a 01 04 05 00 02 01 01 02 01 01 30 16 30 11 0a 01 00 0a 01 00 02 01 02 0a 01 04 05 00 02 01 02 02 01 02 30 16 30 11 0a 01 00 0a 01 00 02 01 03 0a 01 04 05 00 02 01 03 02 01 03 30 16 30 11 0a 01 00 0a 01 00 02 01 04 0a 01 04 05 00 02 01 04 02 01 04

- No.: 275
- Timestamp: 17:16:47:045_0
- RFN: 574
- Chip: 27904
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_SS_1DCH_DCCH_Cfg LINE 9
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 26
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 1a

- No.: 276
- Timestamp: 17:16:47:046_0
- RFN: 574
- Chip: 32768
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_1DCH_DCCH_Cfg LINE 10
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 20
. (RatType)ratType[0] = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . DPCHInfo
. . . . UL_DPCH_Info
. . . . . UL_DPCH_PowerControlInfo
. . . . . . fdd
. . . . . . . (IntegerType)dpcch_PowerOffset[-1] = -40
. . . . . . . (IntegerType)pc_Preamble[-1] = 1
. . . . . . . (IntegerType)sRB_delay[-1] = 7
. . . . . . . PowerControlAlgorithm
. . . . . . . . (IntegerType)algorithm1[-1] = 1
. . . . . modeSpecificInfo
. . . . . . fdd
. . . . . . . (ScramblingCodeType)scramblingCodeType[0] = 1
. . . . . . . (IntegerType)scramblingCode[-1] = 0
. . . . . . . (IntegerType)numberOfDPDCH[-1] = -
. . . . . . . (SpreadingFactor)spreadingFactor[0] = 4
. . . . . . . (BooleanType)tfci_Existence = TRUE
. . . . . . . (IntegerType)numberOfFBI_Bits[-1] = -
. . . . . . . (PuncturingLimit)puncturingLimit[0] = 15
. . . . DL_DPCHInfo
- Constraint:
ca_UL_DPCH_Info
- BinaryMessage:
30 2e 02 01 00 02 01 14 0a 01 00 30 23 30 21 30 1f 30 0c 02 01 d8 02 01 01 02 01 07 02 01 01 30 0f 0a 01 01 02 01 00 0a 01 04 01 01 ff 0a 01 0f

- No.: 280
- Timestamp: 17:16:47:057_0
- RFN: 575
- Chip: 37632
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_1DCH_DCCH_Cfg LINE 11
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 20
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 281
- Timestamp: 17:16:47:059_0
- RFN: 576
- Chip: 6912
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Config_REQ
- Source: ts_SS_1DCH_DCCH_Cfg LINE 12
- Message Structure:
CPHY_TrCH_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 20
. (RatType)ratType[0] = 0
. TrChConfigType
. . (TrChConfigType_list_0)dch[0] = 0
. CphyTrchConfigReq
. . SS_ActivationTime
. . ulconnectedTrCHList
. . . CphyTrchConfigReq_setseq_0
. . . . (IntegerType)trchid[-1] = 5
. . . . (SS_UL_TransportChannelType)ul_TransportChannelType[0] = 0
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size[-1] = 148
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional[0] = 1
. . . . . . (IntegerType)rateMatchingAttribute[-1] = 192
. . . . . . (CRC_Size)crc_Size[0] = 3
. . TFCS
. . . ExplicitTFCS_Configuration
. . . . TFCS_ReconfAdd
. . . . . ctfcSize
. . . . . . ctfc2Bit
. . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . (IntegerType)ctfc2[-1] = 0
. . . . . . . . PowerOffsetInformation
. . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . (IntegerType)ctfc2[-1] = 1
. . . . . . . . PowerOffsetInformation
. . dlconnectedTrCHList
. . TFCS
- Constraint:
ca_DCH_148_TTI_10_UL_InfoActNow
- BinaryMessage:
30 46 02 01 00 02 01 14 0a 01 00 0a 01 00 30 38 05 00 30 26 30 24 02 01 05 0a 01 00 30 1c 30 0e 30 0c 02 02 00 94 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 c0 0a 01 03 30 0c 30 0a 30 03 02 01 00 30 03 02 01 01

- No.: 285
- Timestamp: 17:16:47:067_0
- RFN: 576
- Chip: 37888
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Config_CNF
- Source: ts_SS_1DCH_DCCH_Cfg LINE 13
- Message Structure:
CPHY_TrCH_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 20
- Constraint:
ca_TrChCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 286
- Timestamp: 17:16:47:073_0
- RFN: 577
- Chip: 19712
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_SS_1DCH_DCCH_Cfg LINE 14
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 20
. (RatType)ratType[0] = 0
. configMessage
. . CmacConfigReq
. . . SS_ActivationTime
. . . UE_Info
. . . . U_RNTI
. . . . (BitStringType)c_RNTI[16] = -
. . . TrCHInfo
. . . . ulconnectedTrCHList
. . . . . TrCHInfo_setseq_0
. . . . . . (IntegerType)trchid[-1] = 5
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size[-1] = 148
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional[0] = 1
. . . . . . . . (IntegerType)rateMatchingAttribute[-1] = 192
. . . . . . . . (CRC_Size)crc_Size[0] = 3
. . . . TFCS
. . . . . ExplicitTFCS_Configuration
. . . . . . TFCS_ReconfAdd
. . . . . . . ctfcSize
. . . . . . . . ctfc2Bit
. . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . (IntegerType)ctfc2[-1] = 0
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . (IntegerType)ctfc2[-1] = 1
. . . . . . . . . . PowerOffsetInformation
. . . . dlconnectedTrCHList
. . . . TFCS
. . . TrCH_LogCHMappingList1
. . . . ulconnectedTrCHList
. . . . . TrCH_LogCHMappingList1_setseq_0
. . . . . . (IntegerType)trchid[-1] = 5
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation[0] = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType[0] = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . . . (LogicalChannelType)logicalChannelType[0] = 4
. . . . . . . . (IntegerType)rB_Identity[-1] = 1
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation[0] = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType[0] = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 2
. . . . . . . . . . (LogicalChannelType)logicalChannelType[0] = 4
. . . . . . . . (IntegerType)rB_Identity[-1] = 2
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation[0] = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType[0] = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 3
. . . . . . . . . . (LogicalChannelType)logicalChannelType[0] = 4
. . . . . . . . (IntegerType)rB_Identity[-1] = 3
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation[0] = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType[0] = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 4
. . . . . . . . . . (LogicalChannelType)logicalChannelType[0] = 4
. . . . . . . . (IntegerType)rB_Identity[-1] = 4
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
. . . . dlconnectedTrCHList
- Constraint:
ca_CMAC_CfgInfo
- BinaryMessage:
30 81 9c 02 01 ff 02 01 14 0a 01 00 30 81 90 05 00 30 00 30 33 30 23 30 21 02 01 05 30 1c 30 0e 30 0c 02 02 00 94 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 c0 0a 01 03 30 0c 30 0a 30 03 02 01 00 30 03 02 01 01 30 55 30 53 30 51 02 01 05 30 4c 30 11 30 0c 0a 01 00 0a 01 00 02 01 01 0a 01 04 02 01 01 30 11 30 0c 0a 01 00 0a 01 00 02 01 02 0a 01 04 02 01 02 30 11 30 0c 0a 01 00 0a 01 00 02 01 03 0a 01 04 02 01 03 30 11 30 0c 0a 01 00 0a 01 00 02 01 04 0a 01 04 02 01 04

- No.: 290
- Timestamp: 17:16:47:084_0
- RFN: 578
- Chip: 25088
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_SS_1DCH_DCCH_Cfg LINE 15
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 20
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 14

- No.: 293
- Timestamp: 17:16:47:086_0
- RFN: 578
- Chip: 32000
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB_BCCH_BCH_Cfg LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 246
. . . . . UL_RLC_Mode
. . . . . . UL_TM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . (BooleanType)segmentationIndication = FALSE
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[0] = -
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 1
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_BCCH_Info
- BinaryMessage:
30 1d 02 01 00 02 01 ff 0a 01 00 30 12 30 0b 30 09 02 02 00 f6 30 03 01 01 00 30 03 02 01 01

- No.: 297
- Timestamp: 17:16:47:088_0
- RFN: 579
- Chip: 1792
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB_BCCH_BCH_Cfg LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 300
- Timestamp: 17:16:47:089_0
- RFN: 579
- Chip: 7168
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB_PCCH_Cfg LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -2
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 240
. . . . . UL_RLC_Mode
. . . . . . UL_TM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . (BooleanType)segmentationIndication = FALSE
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[0] = -
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 1
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_PCCH_Info
- BinaryMessage:
30 1d 02 01 00 02 01 fe 0a 01 00 30 12 30 0b 30 09 02 02 00 f0 30 03 01 01 00 30 03 02 01 01

- No.: 304
- Timestamp: 17:16:47:092_0
- RFN: 579
- Chip: 18944
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB_PCCH_Cfg LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 fe

- No.: 307
- Timestamp: 17:16:47:094_0
- RFN: 579
- Chip: 25600
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB0_Cfg LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 0
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 152
. . . . . UL_RLC_Mode
. . . . . . UL_UM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (NoExplicitDiscard)timerBasedNoExplicit[0] = 9
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[0] = -
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 5
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_UM_DL_Info
- BinaryMessage:
30 1d 02 01 00 02 01 00 0a 01 00 30 12 30 0b 30 09 02 02 00 98 30 03 0a 01 09 30 03 02 01 05

- No.: 311
- Timestamp: 17:16:47:096_0
- RFN: 579
- Chip: 33536
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB0_Cfg LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 0
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 00

- No.: 312
- Timestamp: 17:16:47:098_0
- RFN: 580
- Chip: 512
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB0_Cfg LINE 3
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 0
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_TM_RLC_Mode
. . . . . . (BooleanType)segmentationIndication = FALSE
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 166
. . . . . UL_RLC_Mode
. . . . . . UL_TM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . (BooleanType)segmentationIndication = FALSE
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 5
. . . . (IntegerType)dLlogicalChannelIdentity[0] = -
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_TM_UL_Info
- BinaryMessage:
30 22 02 01 00 02 01 00 0a 01 00 30 17 30 10 30 03 01 01 00 30 09 02 02 00 a6 30 03 01 01 00 30 03 02 01 05

- No.: 316
- Timestamp: 17:16:47:104_0
- RFN: 580
- Chip: 26368
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB0_Cfg LINE 4
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 0
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 00

- No.: 319
- Timestamp: 17:16:47:106_0
- RFN: 580
- Chip: 33280
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 1
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 136
. . . . . UL_RLC_Mode
. . . . . . UL_UM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (NoExplicitDiscard)timerBasedNoExplicit[0] = 9
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 1
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 1
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_UM_Info
- BinaryMessage:
30 22 02 01 ff 02 01 01 0a 01 00 30 17 30 0d 05 00 30 09 02 02 00 88 30 03 0a 01 09 30 06 02 01 01 02 01 01

- No.: 323
- Timestamp: 17:16:47:113_0
- RFN: 581
- Chip: 20736
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 324
- Timestamp: 17:16:47:115_0
- RFN: 581
- Chip: 27904
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 3
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 2
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 2
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 2
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 02 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 13 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 02 02 01 02

- No.: 328
- Timestamp: 17:16:47:132_0
- RFN: 583
- Chip: 16384
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 4
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 329
- Timestamp: 17:16:47:134_0
- RFN: 583
- Chip: 23808
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 5
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 3
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 3
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 3
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 03 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 13 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 03 02 01 03

- No.: 333
- Timestamp: 17:16:47:147_0
- RFN: 585
- Chip: 768
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 6
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 3
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 334
- Timestamp: 17:16:47:149_0
- RFN: 585
- Chip: 8192
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 7
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 4
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 4
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 4
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 04 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 13 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 04 02 01 04

- No.: 338
- Timestamp: 17:16:47:165_0
- RFN: 586
- Chip: 24576
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 8
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 4
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 384
- Timestamp: 17:16:47:175_0
- RFN: 587
- Chip: 25088
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 27
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 1b

- No.: 389
- Timestamp: 17:16:47:177_0
- RFN: 587
- Chip: 33280
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendNoSegDefSchedul LINE 2
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 390
- Timestamp: 17:16:47:178_0
- RFN: 587
- Chip: 35840
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendNoSegDefSchedul LINE 3
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 08 02 01 00 02 01 ff 00 00

- No.: 398
- Timestamp: 17:16:47:181_0
- RFN: 588
- Chip: 8960
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 11
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 0b

- No.: 403
- Timestamp: 17:16:47:193_0
- RFN: 589
- Chip: 20224
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB1 LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 404
- Timestamp: 17:16:47:194_0
- RFN: 589
- Chip: 24320
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB1 LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 1
. . . . . . . (BitStringType)sib_Data_variable[-1] = "1100010000000000000001011000100000101000000000100001000000010000000101000000000000000000000011000111010000"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 2
. . . . . . . (BitStringType)sib_Data_variable[-1] = "00000000000000000001"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 1c 02 01 00 02 01 ff 00 0e 21 69 c4 00 05 88 28 02 10 10 14 00 00 0c 74 04 26 00 00 20

- No.: 416
- Timestamp: 17:16:47:198_0
- RFN: 589
- Chip: 37888
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 11
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 0b

- No.: 421
- Timestamp: 17:16:47:204_0
- RFN: 590
- Chip: 22272
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB2 LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 422
- Timestamp: 17:16:47:205_0
- RFN: 590
- Chip: 25856
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB2 LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 1
. . . . . . . (BitStringType)sib_Data_variable[-1] = "1100010000000000000001011000100000101000000000100001000000010000000101000000000000000000000011000111010000"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 2
. . . . . . . (BitStringType)sib_Data_variable[-1] = "00000000000000000001"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 1c 02 01 00 02 01 ff 00 0e 21 69 c4 00 05 88 28 02 10 10 14 00 00 0c 74 04 26 00 00 20

- No.: 434
- Timestamp: 17:16:47:208_0
- RFN: 590
- Chip: 37888
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 10
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 0a

- No.: 439
- Timestamp: 17:16:47:223_0
- RFN: 592
- Chip: 18432
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB3 LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 440
- Timestamp: 17:16:47:224_0
- RFN: 592
- Chip: 21504
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB3 LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 7
. . . . . . . (BitStringType)sib_Data_variable[-1] = "100000101000000010000001"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 3
. . . . . . . (BitStringType)sib_Data_variable[-1] = "010000000000000000000000000000001011001100011000000000100100001000000100011111111111111111111111"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 1b 02 01 00 02 01 ff 00 0e 27 17 82 80 81 1a fa 00 00 00 05 98 c0 12 10 23 ff ff f8

- No.: 452
- Timestamp: 17:16:47:227_0
- RFN: 592
- Chip: 33536
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 26
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 1a

- No.: 457
- Timestamp: 17:16:47:243_0
- RFN: 594
- Chip: 18944
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB4 LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 458
- Timestamp: 17:16:47:244_0
- RFN: 594
- Chip: 22528
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB4 LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 7
. . . . . . . (BitStringType)sib_Data_variable[-1] = "100000101000000010000001"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 4
. . . . . . . (BitStringType)sib_Data_variable[-1] = "0000000000000000000000000000000101100110001100000000010010000100000010001110111"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 19 02 01 00 02 01 ff 00 0e 27 17 82 80 81 22 70 00 00 00 0b 31 80 24 20 47 70

- No.: 475
- Timestamp: 17:16:47:252_0
- RFN: 595
- Chip: 13824
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 23
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 17

- No.: 480
- Timestamp: 17:16:47:254_0
- RFN: 595
- Chip: 24064
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB5 LINE 41
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 481
- Timestamp: 17:16:47:255_0
- RFN: 595
- Chip: 26880
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB5 LINE 42
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 08 02 01 00 02 01 ff 00 00

- No.: 485
- Timestamp: 17:16:47:256_0
- RFN: 595
- Chip: 30976
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 19
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 13

- No.: 490
- Timestamp: 17:16:47:263_0
- RFN: 596
- Chip: 18944
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB5 LINE 44
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 491
- Timestamp: 17:16:47:264_0
- RFN: 596
- Chip: 21760
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB5 LINE 45
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . FirstSegment
. . . . . . (SIB_Type)sib_Type[0] = 5
. . . . . . (IntegerType)seg_Count[-1] = 3
. . . . . . (BitStringType)sib_Data_fixed[222] = "000101010100010000111110000000001111111101000011111111111111110111010010000100001111000000101001000011000000101010100101010110000000000000001100110001011011010101111110001010111010000011111110100000111111101000001111111010"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 25 02 01 00 02 01 ff 00 02 52 15 44 3e 00 ff 43 ff fd d2 10 f0 29 0c 0a a5 58 00 0c c5 b5 7e 2b a0 fe 83 fa 0f e8

- No.: 495
- Timestamp: 17:16:47:265_0
- RFN: 596
- Chip: 25600
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 21
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 15

- No.: 500
- Timestamp: 17:16:47:273_0
- RFN: 597
- Chip: 19200
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB5 LINE 47
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 501
- Timestamp: 17:16:47:274_0
- RFN: 597
- Chip: 22016
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB5 LINE 48
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . SubsequentSegment
. . . . . . (SIB_Type)sib_Type[0] = 5
. . . . . . (IntegerType)segmentIndex[-1] = 1
. . . . . . (BitStringType)sib_Data_fixed[222] = "000011111111010000000000000000001101011000110100010000111111010011100101000001100001000011001010000000110000001110001001000000010110000000000000100000001110000000001000100001100100001010011001000010100000000000110000000100"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 25 02 01 00 02 01 ff 00 04 50 0f f4 00 00 d6 34 43 f4 e5 06 10 ca 03 03 89 01 60 00 80 e0 08 86 42 99 0a 00 30 10

- No.: 505
- Timestamp: 17:16:47:275_0
- RFN: 597
- Chip: 25856
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 22
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 16

- No.: 510
- Timestamp: 17:16:47:283_0
- RFN: 598
- Chip: 17920
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB5 LINE 50
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 512
- Timestamp: 17:16:47:283_2
- RFN: 598
- Chip: 21504
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB5 LINE 52
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . LastSegmentShort
. . . . . . (SIB_Type)sib_Type[0] = 5
. . . . . . (IntegerType)segmentIndex[-1] = 2
. . . . . . (BitStringType)sib_Data_variable[-1] = "010001011100101011010110100000000000011110001000011000000001011011011011011000100000000001000011000010001001010000001011011010000000010000"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 1c 02 01 00 02 01 ff 00 06 51 89 45 ca d6 80 07 88 60 16 db 62 00 43 08 94 0b 68 04 00

- No.: 529
- Timestamp: 17:16:47:287_1
- RFN: 598
- Chip: 35840
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 3
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 03

- No.: 534
- Timestamp: 17:16:47:293_0
- RFN: 599
- Chip: 20224
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB6 LINE 8
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 537
- Timestamp: 17:16:47:294_0
- RFN: 599
- Chip: 23552
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB6:lt_CompleteSIB LINE 4
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 6
. . . . . . . (BitStringType)sib_Data_variable[-1] = "0000001010010001"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 0c 02 01 00 02 01 ff 00 0e 06 0f 02 91

- No.: 542
- Timestamp: 17:16:47:295_1
- RFN: 599
- Chip: 27648
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 5
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 05

- No.: 547
- Timestamp: 17:16:47:302_0
- RFN: 600
- Chip: 18176
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB6 LINE 11
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 548
- Timestamp: 17:16:47:303_0
- RFN: 600
- Chip: 19968
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB6 LINE 12
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 08 02 01 00 02 01 ff 00 00

- No.: 552
- Timestamp: 17:16:47:304_0
- RFN: 600
- Chip: 23296
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 6
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 06

- No.: 557
- Timestamp: 17:16:47:313_0
- RFN: 601
- Chip: 19200
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB6 LINE 14
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 558
- Timestamp: 17:16:47:313_1
- RFN: 601
- Chip: 21504
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB6 LINE 15
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 08 02 01 00 02 01 ff 00 00

- No.: 562
- Timestamp: 17:16:47:314_3
- RFN: 601
- Chip: 25600
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 7
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 07

- No.: 567
- Timestamp: 17:16:47:322_0
- RFN: 602
- Chip: 18176
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB6 LINE 17
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 568
- Timestamp: 17:16:47:323_0
- RFN: 602
- Chip: 20224
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB6 LINE 18
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 08 02 01 00 02 01 ff 00 00

- No.: 576
- Timestamp: 17:16:47:325_3
- RFN: 602
- Chip: 29440
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 2
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 02

- No.: 581
- Timestamp: 17:16:47:333_0
- RFN: 603
- Chip: 20992
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB7 LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 584
- Timestamp: 17:16:47:334_1
- RFN: 603
- Chip: 25856
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB7:lt_CompleteSIB LINE 4
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 7
. . . . . . . (BitStringType)sib_Data_variable[-1] = "100000101000000010000001"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 0d 02 01 00 02 01 ff 00 0e 07 17 82 80 81

- No.: 592
- Timestamp: 17:16:47:338_0
- RFN: 603
- Chip: 38144
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 10
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 0a

- No.: 597
- Timestamp: 17:16:47:353_0
- RFN: 605
- Chip: 19968
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB7:lt_ConcatWithSIB3 LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 598
- Timestamp: 17:16:47:354_0
- RFN: 605
- Chip: 24064
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB7:lt_ConcatWithSIB3 LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 7
. . . . . . . (BitStringType)sib_Data_variable[-1] = "100000101000000010000001"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 3
. . . . . . . (BitStringType)sib_Data_variable[-1] = "010000000000000000000000000000001011001100011000000000100100001000000100011111111111111111111111"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 1b 02 01 00 02 01 ff 00 0e 27 17 82 80 81 1a fa 00 00 00 05 98 c0 12 10 23 ff ff f8

- No.: 606
- Timestamp: 17:16:47:357_0
- RFN: 605
- Chip: 35072
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 18
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 12

- No.: 611
- Timestamp: 17:16:47:363_0
- RFN: 606
- Chip: 19968
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB7:lt_ConcatWithSIB18 LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 612
- Timestamp: 17:16:47:364_0
- RFN: 606
- Chip: 23296
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB7:lt_ConcatWithSIB18 LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 7
. . . . . . . (BitStringType)sib_Data_variable[-1] = "100000101000000010000001"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 26
. . . . . . . (BitStringType)sib_Data_variable[-1] = "100000"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 10 02 01 00 02 01 ff 00 0e 27 17 82 80 81 d0 2c 00

- No.: 620
- Timestamp: 17:16:47:366_3
- RFN: 606
- Chip: 34048
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 26
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 1a

- No.: 625
- Timestamp: 17:16:47:382_0
- RFN: 608
- Chip: 18944
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB7:lt_ConcatWithSIB4 LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 626
- Timestamp: 17:16:47:383_0
- RFN: 608
- Chip: 22528
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB7:lt_ConcatWithSIB4 LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 7
. . . . . . . (BitStringType)sib_Data_variable[-1] = "100000101000000010000001"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 4
. . . . . . . (BitStringType)sib_Data_variable[-1] = "0000000000000000000000000000000101100110001100000000010010000100000010001110111"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 19 02 01 00 02 01 ff 00 0e 27 17 82 80 81 22 70 00 00 00 0b 31 80 24 20 47 70

- No.: 640
- Timestamp: 17:16:47:387_3
- RFN: 608
- Chip: 37888
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 31
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 1f

- No.: 645
- Timestamp: 17:16:47:402_0
- RFN: 610
- Chip: 18688
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB11 LINE 20
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 646
- Timestamp: 17:16:47:403_0
- RFN: 610
- Chip: 21248
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB11 LINE 21
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 08 02 01 00 02 01 ff 00 00

- No.: 650
- Timestamp: 17:16:47:404_1
- RFN: 610
- Chip: 25344
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 29
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 1d

- No.: 655
- Timestamp: 17:16:47:413_0
- RFN: 611
- Chip: 19712
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB11 LINE 23
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 656
- Timestamp: 17:16:47:413_1
- RFN: 611
- Chip: 22784
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB11 LINE 24
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . FirstSegment
. . . . . . (SIB_Type)sib_Type[0] = 11
. . . . . . (IntegerType)seg_Count[-1] = 2
. . . . . . (BitStringType)sib_Data_fixed[222] = "001000001101100100010010000000001000110010000100001000010010010110101000100000100110010001010011000001011001000010100111000010111000010100001000100010001100100101010100000001001010000101001010100001100001001010001000001010"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 25 02 01 00 02 01 ff 00 02 b1 20 d9 12 00 8c 84 21 25 a8 82 64 53 05 90 a7 0b 85 08 88 c9 54 04 a1 4a 86 12 88 28

- No.: 660
- Timestamp: 17:16:47:414_3
- RFN: 611
- Chip: 26880
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 30
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 1e

- No.: 665
- Timestamp: 17:16:47:422_0
- RFN: 612
- Chip: 19456
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB11 LINE 26
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 667
- Timestamp: 17:16:47:423_1
- RFN: 612
- Chip: 23040
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB11 LINE 28
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . LastSegmentShort
. . . . . . (SIB_Type)sib_Type[0] = 11
. . . . . . (IntegerType)segmentIndex[-1] = 1
. . . . . . (BitStringType)sib_Data_variable[-1] = "000100001100001001010010011010101000011000010010101000101100011001010100101010100001001111101000100010000001010010110000100010100001010101111000"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 1c 02 01 00 02 01 ff 00 06 b0 8f 10 c2 52 6a 86 12 a2 c6 54 aa 13 e8 88 14 b0 8a 15 78

- No.: 680
- Timestamp: 17:16:47:426_4
- RFN: 612
- Chip: 34560
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 13
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 0d

- No.: 685
- Timestamp: 17:16:47:442_0
- RFN: 614
- Chip: 18944
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB12 LINE 8
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 688
- Timestamp: 17:16:47:443_2
- RFN: 614
- Chip: 23296
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB12:lt_CompleteSIB LINE 4
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 12
. . . . . . . (BitStringType)sib_Data_variable[-1] = "000000000"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 0c 02 01 00 02 01 ff 00 0e 0c 08 00 00

- No.: 693
- Timestamp: 17:16:47:445_0
- RFN: 614
- Chip: 28160
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 14
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 0e

- No.: 698
- Timestamp: 17:16:47:453_0
- RFN: 615
- Chip: 20480
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB12 LINE 11
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 699
- Timestamp: 17:16:47:453_1
- RFN: 615
- Chip: 23040
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB12 LINE 12
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 08 02 01 00 02 01 ff 00 00

- No.: 703
- Timestamp: 17:16:47:454_3
- RFN: 615
- Chip: 26368
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 15
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 0f

- No.: 708
- Timestamp: 17:16:47:462_0
- RFN: 616
- Chip: 18432
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB12 LINE 14
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 709
- Timestamp: 17:16:47:463_0
- RFN: 616
- Chip: 20736
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB12 LINE 15
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 08 02 01 00 02 01 ff 00 00

- No.: 717
- Timestamp: 17:16:47:465_2
- RFN: 616
- Chip: 30464
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 18
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 12

- No.: 722
- Timestamp: 17:16:47:473_0
- RFN: 617
- Chip: 19968
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB18 LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 723
- Timestamp: 17:16:47:474_0
- RFN: 617
- Chip: 23040
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB18 LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 7
. . . . . . . (BitStringType)sib_Data_variable[-1] = "100000101000000010000001"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 26
. . . . . . . (BitStringType)sib_Data_variable[-1] = "100000"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 10 02 01 00 02 01 ff 00 0e 27 17 82 80 81 d0 2c 00

- No.: 735
- Timestamp: 17:16:47:477_0
- RFN: 617
- Chip: 34048
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 4
. . (IntegerType)sg_POS[-1] = 1
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 04 02 01 01

- No.: 740
- Timestamp: 17:16:47:483_0
- RFN: 618
- Chip: 18688
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSB1_DefSchedul LINE 4
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 743
- Timestamp: 17:16:47:484_0
- RFN: 618
- Chip: 22528
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSB1_DefSchedul:lt_CompleteSIB LINE 4
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 27
. . . . . . . (BitStringType)sib_Data_variable[-1] = "00010000101010001000001100110000010010010100111000101001110100000000010110100010001101110010100010010010"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 17 02 01 00 02 01 ff 00 0e 1b 67 10 a8 83 30 49 4e 29 d0 05 a2 37 28 92

- No.: 761
- Timestamp: 17:16:47:488_0
- RFN: 618
- Chip: 37376
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 3
. . (IntegerType)sg_POS[-1] = 0
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 03 02 01 00

- No.: 766
- Timestamp: 17:16:47:503_0
- RFN: 620
- Chip: 18688
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendMIB LINE 7
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 769
- Timestamp: 17:16:47:504_0
- RFN: 620
- Chip: 23040
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendMIB:lt_CompleteSIB LINE 4
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 0
. . . . . . . (BitStringType)sib_Data_variable[-1] = "0000000000000000010000000010010110101010000100010000000000001000100010110000101000100010110001001000100010100001101000100110100010001110010010010011000100010000"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 1e 02 01 00 02 01 ff 00 0e 00 9f 00 00 40 25 aa 11 00 08 8b 0a 22 c4 88 a1 a2 68 8e 49 31 10

- No.: 786
- Timestamp: 17:16:47:507_0
- RFN: 620
- Chip: 32768
- Event: Send
- PCO: Ut
- Message: MMI_CmdReq
- Source: ts_MMI_UE_SwitchOn LINE 2
- Message Structure:
MMI_CmdReq
. (IA5StringType)cmd[-1] = "Please switch on the UE"
- Constraint:
ca_MMI_CmdReq
- BinaryMessage:
50 6c 65 61 73 65 20 73 77 69 74 63 68 20 6f 6e 20 74 68 65 20 55 45

- No.: 790
- Timestamp: 17:16:47:624_0
- RFN: 632
- Chip: 24064
- Event: Receive
- PCO: Ut
- Message: MMI_CmdCnf
- Source: ts_MMI_UE_SwitchOn LINE 3
- Message Structure:
MMI_CmdCnf
. (BooleanType)result = TRUE
. (IA5StringType)resultString[6] = " OK "
- Constraint:
ca_MMI_CmdCnf
- BinaryMessage:
80 0d 0a 4f 4b 0d 0a

- No.: 810
- Timestamp: 17:16:59:853_0
- RFN: 1855
- Chip: 23040
- Event: Receive
- PCO: TM
- Message: RLC_TR_DATA_IND
- Source: ts_RRC_ConnEst:lt_RcvConnReq LINE 2
- Message Structure:
RLC_TR_DATA_IND
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 0
. tM_message
. . UL_CCCH_Message
. . . IntegrityCheckInfo
. . . UL_CCCH_MessageType
. . . . RRCConnectionRequest
. . . . . InitialUE_Identity
. . . . . . IMSI_GSM_MAP
. . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . (IntegerType)_elem[4] = 1
. . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . (IntegerType)_elem[4] = 1
. . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . (IntegerType)_elem[4] = 1
. . . . . . . (IntegerType)_elem[4] = 2
. . . . . . . (IntegerType)_elem[4] = 3
. . . . . . . (IntegerType)_elem[4] = 4
. . . . . . . (IntegerType)_elem[4] = 5
. . . . . . . (IntegerType)_elem[4] = 6
. . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . (IntegerType)_elem[4] = 6
. . . . . . . (IntegerType)_elem[4] = 3
. . . . . (EstablishmentCause)establishmentCause[5] = 12
. . . . . (ProtocolErrorIndicator)protocolErrorIndicator[1] = 0
. . . . . MeasuredResultsOnRACH
. . . . . v3d0NonCriticalExtensions
- Constraint:
car_RRC_ConnReq
- BinaryMessage:
30 10 02 01 00 02 01 00 20 90 01 01 01 23 45 60 63 60

- No.: 814
- Timestamp: 17:16:59:861_0
- RFN: 1856
- Chip: 15872
- Event: Send
- PCO: UM
- Message: RLC_UM_DATA_REQ
- Source: ts_RRC_ConnEst:lt_Send_ConnSetUp LINE 22
- Message Structure:
RLC_UM_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 0
. uM_message
. . DL_CCCH_Message
. . . IntegrityCheckInfo
. . . DL_CCCH_MessageType
. . . . RRCConnectionSetup
. . . . . r3
. . . . . . RRCConnectionSetup_r3_IEs
. . . . . . . InitialUE_Identity
. . . . . . . . IMSI_GSM_MAP
. . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . (IntegerType)_elem[4] = 1
. . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . (IntegerType)_elem[4] = 1
. . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . (IntegerType)_elem[4] = 1
. . . . . . . . . (IntegerType)_elem[4] = 2
. . . . . . . . . (IntegerType)_elem[4] = 3
. . . . . . . . . (IntegerType)_elem[4] = 4
. . . . . . . . . (IntegerType)_elem[4] = 5
. . . . . . . . . (IntegerType)_elem[4] = 6
. . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . (IntegerType)_elem[4] = 6
. . . . . . . . . (IntegerType)_elem[4] = 3
. . . . . . . (IntegerType)rrc_TransactionIdentifier[-1] = 0
. . . . . . . (IntegerType)activationTime[-1] = -
. . . . . . . U_RNTI
. . . . . . . . (BitStringType)srnc_Identity[12] = "000000000001"
. . . . . . . . (BitStringType)s_RNTI[20] = "00000000000000000001"
. . . . . . . (BitStringType)new_c_RNTI[16] = -
. . . . . . . (RRC_StateIndicator)rrc_StateIndicator[0] = 0
. . . . . . . (IntegerType)utran_DRX_CycleLengthCoeff[-1] = 9
. . . . . . . CapabilityUpdateRequirement
. . . . . . . . (BooleanType)ue_RadioCapabilityFDDUpdateRequirement = TRUE
. . . . . . . . (BooleanType)ue_RadioCapabilityTDDUpdateRequirement = FALSE
. . . . . . . . SystemSpecificCapUpdateReqList
. . . . . . . . . (SystemSpecificCapUpdateReq)_elem[0] = 0
. . . . . . . SRB_InformationSetupList2
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity[-1] = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_UM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 1
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex[-1] = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 1
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity[-1] = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 2
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 2
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 2
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 2
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex[-1] = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 2
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 2
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity[-1] = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 3
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 3
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 3
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 3
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex[-1] = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 3
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 3
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity[-1] = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 4
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 4
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 4
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 4
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex[-1] = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 4
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 4
. . . . . . . UL_CommonTransChInfo
. . . . . . . . TFC_Subset
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . TFCS
. . . . . . . . . . . ExplicitTFCS_Configuration
. . . . . . . . . . . . TFCS_ReconfAdd
. . . . . . . . . . . . . ctfcSize
. . . . . . . . . . . . . . ctfc2Bit
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . . . . . . . (IntegerType)ctfc2[-1] = 0
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . . . . . . . (IntegerType)ctfc2[-1] = 1
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC[-1] = 11
. . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaD[-1] = 15
. . . . . . . . . . . . . . . . . . . (IntegerType)referenceTFC_ID[-1] = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . UL_AddReconfTransChInfoList
. . . . . . . . UL_AddReconfTransChInformation
. . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType[0] = 0
. . . . . . . . . (IntegerType)transportChannelIdentity[-1] = 5
. . . . . . . . . TransportFormatSet
. . . . . . . . . . DedicatedTransChTFS
. . . . . . . . . . . tti
. . . . . . . . . . . . DedicatedDynamicTF_InfoList
. . . . . . . . . . . . . DedicatedDynamicTF_Info
. . . . . . . . . . . . . . rlc_Size
. . . . . . . . . . . . . . . BitModeRLC_SizeInfo
. . . . . . . . . . . . . . . . sizeType2
. . . . . . . . . . . . . . . . . (IntegerType)part1[-1] = 2
. . . . . . . . . . . . . . . . . (IntegerType)part2[-1] = -
. . . . . . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . LogicalChannelList
. . . . . . . . . . . SemistaticTF_Information
. . . . . . . . . . . . ChannelCodingType
. . . . . . . . . . . . . (CodingRate)convolutional[0] = 1
. . . . . . . . . . . . (IntegerType)rateMatchingAttribute[-1] = 192
. . . . . . . . . . . . (CRC_Size)crc_Size[0] = 3
. . . . . . . DL_CommonTransChInfo
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . dl_Parameters
. . . . . . . DL_AddReconfTransChInfoList
. . . . . . . . DL_AddReconfTransChInformation
. . . . . . . . . (DL_TrCH_Type)dl_TransportChannelType[0] = 0
. . . . . . . . . (IntegerType)dl_transportChannelIdentity[-1] = 10
. . . . . . . . . tfs_SignallingMode
. . . . . . . . . . UL_TransportChannelIdentity
. . . . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType[0] = 0
. . . . . . . . . . . (IntegerType)ul_TransportChannelIdentity[-1] = 5
. . . . . . . . . QualityTarget
. . . . . . . . . . (IntegerType)bler_QualityValue[-1] = -20
. . . . . . . . . TM_SignallingInfo
. . . . . . . FrequencyInfo
. . . . . . . (IntegerType)maxAllowedUL_TX_Power[-1] = -
. . . . . . . UL_ChannelRequirement
. . . . . . . . UL_DPCH_Info
. . . . . . . . . UL_DPCH_PowerControlInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (IntegerType)dpcch_PowerOffset[-1] = -40
. . . . . . . . . . . (IntegerType)pc_Preamble[-1] = 1
. . . . . . . . . . . (IntegerType)sRB_delay[-1] = 7
. . . . . . . . . . . PowerControlAlgorithm
. . . . . . . . . . . . (IntegerType)algorithm1[-1] = 1
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (ScramblingCodeType)scramblingCodeType[0] = 1
. . . . . . . . . . . (IntegerType)scramblingCode[-1] = 0
. . . . . . . . . . . (IntegerType)numberOfDPDCH[-1] = -
. . . . . . . . . . . (SpreadingFactor)spreadingFactor[0] = 4
. . . . . . . . . . . (BooleanType)tfci_Existence = TRUE
. . . . . . . . . . . (IntegerType)numberOfFBI_Bits[-1] = -
. . . . . . . . . . . (PuncturingLimit)puncturingLimit[0] = 15
. . . . . . . DL_CommonInformation
. . . . . . . . DL_DPCH_InfoCommon
. . . . . . . . . cfnHandling
. . . . . . . . . . initialise
. . . . . . . . . . . (IntegerType)cfntargetsfnframeoffset[-1] = -
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . DL_DPCH_PowerControlInfo
. . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . (DPC_Mode)dpc_Mode[0] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPilot_pdpdch[-1] = 0
. . . . . . . . . . . Dl_rate_matching_restriction
. . . . . . . . . . . SF512_AndPilot
. . . . . . . . . . . . (PilotBits128)sfd128[0] = 0
. . . . . . . . . . . (PositionFixedOrFlexible)positionFixedOrFlexible[0] = 0
. . . . . . . . . . . (BooleanType)tfci_Existence = FALSE
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . (IntegerType)defaultDPCH_OffsetValue[-1] = 459
. . . . . . . . . . DPCH_CompressedModeInfo
. . . . . . . . . . (TX_DiversityMode)tx_DiversityMode[0] = 0
. . . . . . . . . . SSDT_Information
. . . . . . . DL_InformationPerRL_List
. . . . . . . . DL_InformationPerRL
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . PrimaryCPICH_Info
. . . . . . . . . . . . (IntegerType)primaryScramblingCode[-1] = 100
. . . . . . . . . . . PDSCH_SHO_DCH_Info
. . . . . . . . . . . PDSCH_CodeMapping
. . . . . . . . . DL_DPCH_InfoPerRL
. . . . . . . . . . fdd
. . . . . . . . . . . (PCPICH_UsageForChannelEst)pCPICH_UsageForChannelEst[0] = 0
. . . . . . . . . . . (IntegerType)dpch_FrameOffset[-1] = 18
. . . . . . . . . . . SecondaryCPICH_Info
. . . . . . . . . . . DL_ChannelisationCodeList
. . . . . . . . . . . . DL_ChannelisationCode
. . . . . . . . . . . . . (IntegerType)secondaryScramblingCode[-1] = 1
. . . . . . . . . . . . . SF512_AndCodeNumber
. . . . . . . . . . . . . . (IntegerType)sf128[-1] = 0
. . . . . . . . . . . . . (ScramblingCodeChange)scramblingCodeChange[0] = 1
. . . . . . . . . . . (IntegerType)tpc_CombinationIndex[-1] = 0
. . . . . . . . . . . (SSDT_CellIdentity)ssdt_CellIdentity[0] = -
. . . . . . . . . . . (ClosedLoopTimingAdjMode)closedLoopTimingAdjMode[0] = -
. . . . . . . . . SCCPCH_InfoForFACH
. . . . . . laterNonCriticalExtensions
. (BooleanType)specialLI = TRUE
- Constraint:
cas_RRC_ConnSetup
- BinaryMessage:
30 78 02 01 00 02 01 00 30 e7 12 00 20 20 24 68 ac 0c 60 00 80 00 09 b0 4d 27 42 02 11 21 a8 40 00 50 33 d1 c8 d9 34 cf 93 89 ce 84 14 a2 47 51 80 02 a2 67 a3 91 b2 69 9f 27 13 9d 08 4a 44 96 a5 00 09 48 cf 47 23 64 d3 3e 4e 27 3a 10 d6 89 3d 4e 00 1a 99 00 00 c4 a5 7e 00 40 01 10 44 77 ec c1 13 12 b4 a8 f4 40 00 00 27 f2 01 42 9c b0 40 c8 01 21 85 01 00 01 01 ff

- No.: 835
- Timestamp: 17:16:59:883_5
- RFN: 1858
- Chip: 25600
- Event: Start Timer
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 3
- Message Structure:
no details available
- Constraint:
t_WaitMS (13500 Ms)
- BinaryMessage:

- No.: 842
- Timestamp: 17:17:00:084_1
- RFN: 1878
- Chip: 28416
- Event: Receive
- PCO: CPHY
- Message: CPHY_Sync_IND
- Source: RRC_DefConnEst LINE 5
- Message Structure:
CPHY_Sync_IND
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 20
- Constraint:
ca_SyncInd
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 843
- Timestamp: 17:17:00:085_0
- RFN: 1878
- Chip: 29184
- Event: Cancel Timer
- Source: RRC_DefConnEst LINE 5
- Message Structure:
no details available
- Constraint:
t_T312
- BinaryMessage:

- No.: 844
- Timestamp: 17:17:00:085_1
- RFN: 1878
- Chip: 29952
- Event: Default
- Source: RRC_DefConnEst LINE 0
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 845
- Timestamp: 17:17:00:085_2
- RFN: 1878
- Chip: 30208
- Event: Default
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 852
- Timestamp: 17:17:00:186_0
- RFN: 1888
- Chip: 35328
- Event: Receive
- PCO: AM
- Message: RLC_AM_DATA_IND
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
RLC_AM_DATA_IND
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 2
. IntegrityResult
. . (IntegrityStatus)integrityUsed[0] = 4294967296
. aM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . UL_DCCH_MessageType
. . . . RRCConnectionSetupComplete
. . . . . (IntegerType)rrc_TransactionIdentifier[2] = 0
. . . . . STARTList
. . . . . . STARTSingle
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity[1] = 1
. . . . . . . (BitStringType)start_Value[20] = "00000000000000000010"
. . . . . . STARTSingle
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity[1] = 0
. . . . . . . (BitStringType)start_Value[20] = "00000000000000000010"
. . . . . UE_RadioAccessCapability
. . . . . . (AccessStratumReleaseIndicator)accessStratumReleaseIndicator[0] = 0
. . . . . . PDCP_Capability
. . . . . . . (BooleanType)losslessSRNS_RelocationSupport = FALSE
. . . . . . . supportForRfc2507
. . . . . . . . (MaxHcContextSpace)supported[3] = 4
. . . . . . RLC_Capability
. . . . . . . (TotalRLC_AM_BufferSize)totalRLC_AM_BufferSize[3] = 2
. . . . . . . (MaximumRLC_WindowSize)maximumRLC_WindowSize[1] = 0
. . . . . . . (MaximumAM_EntityNumberRLC_Cap)maximumAM_EntityNumber[3] = 3
. . . . . . TransportChannelCapability
. . . . . . . DL_TransChCapability
. . . . . . . . (MaxNoBits)maxNoBitsReceived[4] = 7
. . . . . . . . (MaxNoBits)maxConvCodeBitsReceived[4] = 1
. . . . . . . . TurboSupport
. . . . . . . . . (MaxNoBits)supported[4] = 7
. . . . . . . . (MaxSimultaneousTransChsDL)maxSimultaneousTransChs[2] = 1
. . . . . . . . (IntegerType)maxSimultaneousCCTrCH_Count[3] = 1
. . . . . . . . (MaxTransportBlocksDL)maxReceivedTransportBlocks[4] = 3
. . . . . . . . (MaxNumberOfTFC_DL)maxNumberOfTFC[4] = 5
. . . . . . . . (MaxNumberOfTF)maxNumberOfTF[3] = 1
. . . . . . . UL_TransChCapability
. . . . . . . . (MaxNoBits)maxNoBitsTransmitted[4] = 3
. . . . . . . . (MaxNoBits)maxConvCodeBitsTransmitted[4] = 1
. . . . . . . . TurboSupport
. . . . . . . . . (MaxNoBits)supported[4] = 3
. . . . . . . . (MaxSimultaneousTransChsUL)maxSimultaneousTransChs[3] = 2
. . . . . . . . modeSpecificInfo
. . . . . . . . (MaxTransportBlocksUL)maxTransmittedBlocks[4] = 4
. . . . . . . . (MaxNumberOfTFC_UL)maxNumberOfTFC[4] = 5
. . . . . . . . (MaxNumberOfTF)maxNumberOfTF[3] = 0
. . . . . . RF_Capability
. . . . . . . fddRF_Capability
. . . . . . . . (IntegerType)ue_PowerClass[2] = 4
. . . . . . . . (TxRxFrequencySeparation)txRxFrequencySeparation[2] = 0
. . . . . . . tddRF_Capability
. . . . . . PhysicalChannelCapability
. . . . . . . fddPhysChCapability
. . . . . . . . DL_PhysChCapabilityFDD
. . . . . . . . . (IntegerType)maxNoDPCH_PDSCH_Codes[3] = 1
. . . . . . . . . (MaxNoPhysChBitsReceived)maxNoPhysChBitsReceived[4] = 6
. . . . . . . . . (BooleanType)supportForSF_512 = FALSE
. . . . . . . . . (BooleanType)supportOfPDSCH = FALSE
. . . . . . . . . SimultaneousSCCPCH_DPCH_Reception
. . . . . . . . UL_PhysChCapabilityFDD
. . . . . . . . . (MaxNoDPDCH_BitsTransmitted)maxNoDPDCH_BitsTransmitted[4] = 3
. . . . . . . . . (BooleanType)supportOfPCPCH = FALSE
. . . . . . . tddPhysChCapability
. . . . . . UE_MultiModeRAT_Capability
. . . . . . . MultiRAT_Capability
. . . . . . . . (BooleanType)supportOfGSM = FALSE
. . . . . . . . (BooleanType)supportOfMulticarrier = FALSE
. . . . . . . (MultiModeCapability)multiModeCapability[2] = 1
. . . . . . SecurityCapability
. . . . . . . (BitStringType)cipheringAlgorithmCap[16] = '0000000000000011'B
. . . . . . . (BitStringType)integrityProtectionAlgorithmCap[16] = '0000000000000010'B
. . . . . . UE_Positioning_Capability
. . . . . . . (BooleanType)standaloneLocMethodsSupported = FALSE
. . . . . . . (BooleanType)ue_BasedOTDOA_Supported = FALSE
. . . . . . . (NetworkAssistedGPS_Supported)networkAssistedGPS_Supported[2] = 3
. . . . . . . (BooleanType)supportForUE_GPS_TimingOfCellFrames = FALSE
. . . . . . . (BooleanType)supportForIPDL = FALSE
. . . . . . MeasurementCapability
. . . . . . . CompressedModeMeasCapability
. . . . . . . . (BooleanType)fdd_Measurements = TRUE
. . . . . . . . (BooleanType)tdd_Measurements = -
. . . . . . . . GSM_Measurements
. . . . . . . . . (BooleanType)gsm900 = TRUE
. . . . . . . . . (BooleanType)dcs1800 = TRUE
. . . . . . . . . (BooleanType)gsm1900 = TRUE
. . . . . . . . (BooleanType)multiCarrierMeasurements = FALSE
. . . . . . . CompressedModeMeasCapability
. . . . . . . . (BooleanType)fdd_Measurements = TRUE
. . . . . . . . (BooleanType)tdd_Measurements = -
. . . . . . . . GSM_Measurements
. . . . . . . . . (BooleanType)gsm900 = TRUE
. . . . . . . . . (BooleanType)dcs1800 = TRUE
. . . . . . . . . (BooleanType)gsm1900 = TRUE
. . . . . . . . (BooleanType)multiCarrierMeasurements = FALSE
. . . . . v370NonCriticalExtensions
- Constraint:
car_RRC_ConnSetupCmpl
- BinaryMessage:
30 27 02 01 ff 02 01 02 0a 05 01 00 00 00 00 4a 0c 00 00 80 00 05 62 37 1b a0 d4 98 cd 11 45 90 60 61 00 03 00 02 31 f9 f8

- No.: 853
- Timestamp: 17:17:00:188_0
- RFN: 1889
- Chip: 4096
- Event: Cancel Timer
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
t_WaitMS
- BinaryMessage:

- No.: 854
- Timestamp: 17:17:00:188_1
- RFN: 1889
- Chip: 4352
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 873
- Timestamp: 17:17:00:205_0
- RFN: 1890
- Chip: 31488
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_GMM_IdleUpdated:lt_IdleUpdated_NMO_I LINE 10
- Message Structure:
RRC_DataInd
. (IntegerType)cellId[0] = -1
. (SS_RB_Identity)rB_Id[0] = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain[0] = 0
. (START_Value)start[20] = '00000000000000000010'B
. LOCATIONUPDATINGREQUEST
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)mMProtocolDiscriminator[4] = '0101'B
. . (MsgType)msgType[8] = '00001000'B
. . CiphKeySeqNum
. . . (B1)spare1[1] = '0'B
. . . (KeySeq)keySeq[3] = '111'B
. . LocUpdType
. . . (B1)fOR[1] = '0'B
. . . (B1)spare1[1] = '0'B
. . . (B2)lUT[2] = '00'B
. . LocAreaId_v
. . . (OctetStringType)plmn[3] = '32F451'O
. . . (OctetStringType)lac[2] = 'FFFE'O
. . MS_Clsmk1
. . . (B1)spare1[1] = '0'B
. . . (B2)revLvl[2] = '10'B
. . . (B1)eSIND[1] = '0'B
. . . (B1)a5_1[1] = '1'B
. . . (B3)rFPwrCap[3] = '111'B
. . MS_Identity_lv
. . . (Length)iel[1] = '08'O
. . . (B4)iDigit1[4] = '0000'B
. . . (B1)oddEvenInd[1] = '1'B
. . . (B3)typeOfId[3] = '001'B
. . . (OctetStringType)otherDigits[7] = '10101032540636'O
. . MS_Clsmk2
. . . (IEI8)iei[8] = '00110011'B
. . . (Length)iel[1] = '03'O
. . . (B1)spare1_1[1] = '0'B
. . . (B2)revLvl[2] = '10'B
. . . (B1)eSIND[1] = '0'B
. . . (B1)a5_1[1] = '1'B
. . . (B3)rFPwrCap[3] = '111'B
. . . (B1)spare1_2[1] = '0'B
. . . (B1)pSCap[1] = '0'B
. . . (B2)sSSI[2] = '01'B
. . . (B1)sMCap[1] = '1'B
. . . (B1)vBS[1] = '0'B
. . . (B1)vGCS[1] = '0'B
. . . (B1)fC[1] = '0'B
. . . (B1)cM3[1] = '1'B
. . . (B1)spare1_3[1] = '0'B
. . . (B1)lCSVA[1] = '1'B
. . . (B1)uCS2[1] = '0'B
. . . (B1)soLSA[1] = '0'B
. . . (B1)cMSP[1] = '0'B
. . . (B1)a5_3[1] = '0'B
. . . (B1)a5_2[1] = '0'B
- Constraint:
car_InitDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 00 03 04 04 00 00 20 05 08 70 32 f4 51 ff fe 4f 08 09 10 10 10 32 54 06 36 33 03 4f 18 a0

- No.: 909
- Timestamp: 17:17:00:217_0
- RFN: 1892
- Chip: 3328
- Event: Send
- PCO: Dc
- Message: RRC_DataReq
- Source: ts_MM_Authentication LINE 2
- Message Structure:
RRC_DataReq
. (IntegerType)cellId[-1] = -1
. (SS_RB_Identity)rB_Id[-1] = 3
. (LogicChGERAN)ch[-1] = -
. (SapId)sapId[1] = -
. (SS_CN_DomainIdentity)cN_Domain[-1] = 0
. AUTHENTICATIONREQUEST
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)mMProtocolDiscriminator[4] = '0101'B
. . (MsgType)msgType[8] = '00010010'B
. . (B4)spare4[4] = '0000'B
. . CiphKeySeqNum
. . . (B1)spare1[1] = '0'B
. . . (KeySeq)keySeq[3] = '000'B
. . (MM_RAND)rAND[128] = '01010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101'B
. . AUTN
. . . (IEI8)iei[8] = '00100000'B
. . . (Length)iel[1] = '10'O
. . . (BitStringType)aUTN[128] = '01010110010100010101000001010011010100100101110100000000000000000101010101010100010101110101011001010001010100000101001101010010'B
- Constraint:
ca_DataReq
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 00 05 12 00 55 55 55 55 55 55 55 55 55 55 55 55 55 55 55 55 20 10 56 51 50 53 52 5d 00 00 55 54 57 56 51 50 53 52

- No.: 913
- Timestamp: 17:17:00:495_0
- RFN: 1919
- Chip: 30720
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_MM_Authentication LINE 3
- Message Structure:
RRC_DataInd
. (IntegerType)cellId[0] = -1
. (SS_RB_Identity)rB_Id[0] = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain[0] = 0
. (START_Value)start[0] = -
. AUTHENTICATIONRESPONSE
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)mMProtocolDiscriminator[4] = '0101'B
. . (MsgType)msgType[8] = '01010100'B
. . (AuthRsp)authRsp[32] = '01010101010101000101011101010110'B
. . AuthRspExt
. . . (IEI8)iei[8] = '00100001'B
. . . (Length)iel[1] = '0C'O
. . . (BitStringType)rES[96] = '010100010101000001010011010100100101110101011100010111110101111001011001010110000101101101011010'B
- Constraint:
car_UplinkDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 00 05 54 55 54 57 56 21 0c 51 50 53 52 5d 5c 5f 5e 59 58 5b 5a

- No.: 955
- Timestamp: 17:17:00:500_4
- RFN: 1920
- Chip: 15104
- Event: Send
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_REQ
- Source: ts_SS_DownloadSecurityKey:lt_DownloadKeyCRLC LINE 1
- Message Structure:
CRLC_SecurityMode_Config_REQ
. (IntegerType)cellId[-1] = -1
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity[0] = 0
. . (BitStringType)startValue[20] = "00000000000000000000"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = '01010111010101100101000101010000010100110101001001011101010111000101111101011110010110010101100001011011010110100101010101010100'B
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CRLC_SecurityModeCfgReq
- BinaryMessage:
30 21 02 01 ff 30 1c 0a 01 00 03 04 04 00 00 00 03 11 00 57 56 51 50 53 52 5d 5c 5f 5e 59 58 5b 5a 55 54

- No.: 956
- Timestamp: 17:17:00:501_0
- RFN: 1920
- Chip: 17152
- Event: Receive
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_CNF
- Source: ts_SS_DownloadSecurityKey:lt_DownloadKeyCRLC LINE 2
- Message Structure:
CRLC_SecurityMode_Config_CNF
. (IntegerType)cellId[0] = -1
- Constraint:
ca_CRLC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 963
- Timestamp: 17:17:00:502_3
- RFN: 1920
- Chip: 21760
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 1
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 0
. (IntegerType)count_I_LSB_UL[-1] = -
. (IntegerType)count_I_LSB_DL[-1] = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 00 02 01 00 02 01 00

- No.: 964
- Timestamp: 17:17:00:503_0
- RFN: 1920
- Chip: 23552
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 2
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 0
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 00 02 01 00

- No.: 965
- Timestamp: 17:17:00:503_1
- RFN: 1920
- Chip: 25344
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 3
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 1
. (IntegerType)count_I_LSB_UL[-1] = -
. (IntegerType)count_I_LSB_DL[-1] = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 01 02 01 00

- No.: 966
- Timestamp: 17:17:00:504_0
- RFN: 1920
- Chip: 26880
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 4
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 1
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 967
- Timestamp: 17:17:00:504_1
- RFN: 1920
- Chip: 28672
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 5
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 2
. (IntegerType)count_I_LSB_UL[-1] = -
. (IntegerType)count_I_LSB_DL[-1] = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 02 02 01 00

- No.: 968
- Timestamp: 17:17:00:504_2
- RFN: 1920
- Chip: 30208
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 6
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 2
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 969
- Timestamp: 17:17:00:505_0
- RFN: 1920
- Chip: 32256
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 7
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 3
. (IntegerType)count_I_LSB_UL[-1] = -
. (IntegerType)count_I_LSB_DL[-1] = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 03 02 01 00

- No.: 970
- Timestamp: 17:17:00:505_1
- RFN: 1920
- Chip: 33792
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 8
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 3
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 971
- Timestamp: 17:17:00:506_0
- RFN: 1920
- Chip: 35840
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 9
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 4
. (IntegerType)count_I_LSB_UL[-1] = -
. (IntegerType)count_I_LSB_DL[-1] = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 04 02 01 00

- No.: 972
- Timestamp: 17:17:00:506_1
- RFN: 1920
- Chip: 37376
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 10
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 4
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 976
- Timestamp: 17:17:00:507_2
- RFN: 1921
- Chip: 2816
- Event: Send
- PCO: CRLC
- Message: CRLC_Integrity_Activate_REQ
- Source: ts_CRLC_DL_Integrity LINE 1
- Message Structure:
CRLC_Integrity_Activate_REQ
. (IntegerType)cellId[-1] = -1
. (CN_DomainIdentity)cn_DomainIdentity[0] = 0
. IntegrityActivationInfo
. . IntegrityProtectionModeInfo
. . . IntegrityProtectionModeCommand
. . . . startIntegrityProtection
. . . . . (BitStringType)integrityProtInitNumber[32] = "00000000000000000000000000000001"
. . . (IntegrityProtectionAlgorithm)integrityProtectionAlgorithm[0] = 0
- Constraint:
ca_CRLC_DL_IntegrityActivateReq
- BinaryMessage:
30 14 02 01 ff 0a 01 00 30 0c 30 07 03 05 00 00 00 00 01 0a 01 00

- No.: 977
- Timestamp: 17:17:00:508_0
- RFN: 1921
- Chip: 4608
- Event: Receive
- PCO: CRLC
- Message: CRLC_Integrity_Activate_CNF
- Source: ts_CRLC_DL_Integrity LINE 2
- Message Structure:
CRLC_Integrity_Activate_CNF
. (IntegerType)cellId[0] = -1
- Constraint:
ca_CRLC_IntegrityActivateCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 984
- Timestamp: 17:17:00:509_1
- RFN: 1921
- Chip: 9984
- Event: Send
- PCO: CRLC
- Message: CRLC_Integrity_Activate_REQ
- Source: ts_RB2_UL_IntegrityActivate LINE 1
- Message Structure:
CRLC_Integrity_Activate_REQ
. (IntegerType)cellId[-1] = -1
. (CN_DomainIdentity)cn_DomainIdentity[0] = 0
. IntegrityActivationInfo
. . IntegrityProtActivationInfoList
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity[-1] = 2
. . . . (IntegerType)rrc_MessageSequenceNumber[-1] = 0
- Constraint:
ca_CRLC_UL_IntegrityActivateReq
- BinaryMessage:
30 10 02 01 ff 0a 01 00 30 08 30 06 02 01 02 02 01 00

- No.: 985
- Timestamp: 17:17:00:510_0
- RFN: 1921
- Chip: 12288
- Event: Receive
- PCO: CRLC
- Message: CRLC_Integrity_Activate_CNF
- Source: ts_RB2_UL_IntegrityActivate LINE 2
- Message Structure:
CRLC_Integrity_Activate_CNF
. (IntegerType)cellId[0] = -1
- Constraint:
ca_CRLC_IntegrityActivateCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 992
- Timestamp: 17:17:00:511_0
- RFN: 1921
- Chip: 18688
- Event: Send
- PCO: AM
- Message: RLC_AM_DATA_REQ
- Source: ts_RRC_Security:lt_SendSecurityModeCommand LINE 16
- Message Structure:
RLC_AM_DATA_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 2
. AmConfirmationRequest
. aM_message
. . DL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00000000000000000000000000000000"
. . . . (IntegerType)rrc_MessageSequenceNumber[-1] = 0
. . . DL_DCCH_MessageType
. . . . SecurityModeCommand
. . . . . r3
. . . . . . SecurityModeCommand_r3_IEs
. . . . . . . (IntegerType)rrc_TransactionIdentifier[-1] = 0
. . . . . . . SecurityCapability
. . . . . . . . (BitStringType)cipheringAlgorithmCap[16] = '0000000000000011'B
. . . . . . . . (BitStringType)integrityProtectionAlgorithmCap[16] = '0000000000000010'B
. . . . . . . CipheringModeInfo
. . . . . . . IntegrityProtectionModeInfo
. . . . . . . . IntegrityProtectionModeCommand
. . . . . . . . . startIntegrityProtection
. . . . . . . . . . (BitStringType)integrityProtInitNumber[32] = "00000000000000000000000000000001"
. . . . . . . . (IntegrityProtectionAlgorithm)integrityProtectionAlgorithm[0] = 0
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity[0] = 0
. . . . . . . InterRAT_UE_SecurityCapList
. . . . . . laterNonCriticalExtensions
- Constraint:
cas_RRC_SecModeCmd
- BinaryMessage:
30 17 02 01 ff 02 01 02 05 00 80 00 00 00 04 04 00 01 80 01 40 00 00 00 20

- No.: 1001
- Timestamp: 17:17:00:634_0
- RFN: 1933
- Chip: 31488
- Event: Receive
- PCO: AM
- Message: RLC_AM_DATA_IND
- Source: ts_RRC_Security:lt_StartSecurity_UE LINE 8
- Message Structure:
RLC_AM_DATA_IND
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 2
. IntegrityResult
. . (IntegrityStatus)integrityUsed[0] = 0
. aM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "10000001100000001110110111011101"
. . . . (IntegerType)rrc_MessageSequenceNumber[4] = 1
. . . UL_DCCH_MessageType
. . . . SecurityModeComplete
. . . . . (IntegerType)rrc_TransactionIdentifier[2] = 0
. . . . . IntegrityProtActivationInfo
. . . . . . RRC_MessageSequenceNumberList
. . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . (IntegerType)_elem[4] = 0
. . . . . laterNonCriticalExtensions
- Constraint:
car_RRC_SecModeCmpl
- BinaryMessage:
30 12 02 01 ff 02 01 02 0a 01 00 c0 c0 76 ee 8d 21 00 00 00

- No.: 1002
- Timestamp: 17:17:00:635_0
- RFN: 1933
- Chip: 33024
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_Security:lt_StartSecurity_UE LINE 8
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1004
- Timestamp: 17:17:00:635_2
- RFN: 1933
- Chip: 36096
- Event: Send
- PCO: CRLC
- Message: CRLC_Integrity_Activate_REQ
- Source: ts_CRLC_UL_Integrity LINE 1
- Message Structure:
CRLC_Integrity_Activate_REQ
. (IntegerType)cellId[-1] = -1
. (CN_DomainIdentity)cn_DomainIdentity[0] = 0
. IntegrityActivationInfo
. . IntegrityProtActivationInfoList
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity[-1] = 0
. . . . (IntegerType)rrc_MessageSequenceNumber[-1] = 0
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity[-1] = 1
. . . . (IntegerType)rrc_MessageSequenceNumber[-1] = 0
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity[-1] = 3
. . . . (IntegerType)rrc_MessageSequenceNumber[-1] = 0
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity[-1] = 4
. . . . (IntegerType)rrc_MessageSequenceNumber[-1] = 0
- Constraint:
ca_CRLC_UL_IntegrityActivateReq
- BinaryMessage:
30 28 02 01 ff 0a 01 00 30 20 30 06 02 01 00 02 01 00 30 06 02 01 01 02 01 00 30 06 02 01 03 02 01 00 30 06 02 01 04 02 01 00

- No.: 1005
- Timestamp: 17:17:00:636_0
- RFN: 1933
- Chip: 38144
- Event: Receive
- PCO: CRLC
- Message: CRLC_Integrity_Activate_CNF
- Source: ts_CRLC_UL_Integrity LINE 2
- Message Structure:
CRLC_Integrity_Activate_CNF
. (IntegerType)cellId[0] = -1
- Constraint:
ca_CRLC_IntegrityActivateCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1010
- Timestamp: 17:17:00:638_1
- RFN: 1934
- Chip: 4352
- Event: Send
- PCO: Dc
- Message: RRC_DataReq
- Source: ts_GMM_IdleUpdated:lt_IdleUpdated_NMO_I LINE 14
- Message Structure:
RRC_DataReq
. (IntegerType)cellId[-1] = -1
. (SS_RB_Identity)rB_Id[-1] = 3
. (LogicChGERAN)ch[-1] = -
. (SapId)sapId[1] = -
. (SS_CN_DomainIdentity)cN_Domain[-1] = 0
. LOCATIONUPDATINGACCEPT
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)mMProtocolDiscriminator[4] = '0101'B
. . (MsgType)msgType[8] = '00000010'B
. . LocAreaId_v
. . . (OctetStringType)plmn[3] = '00F110'O
. . . (OctetStringType)lac[2] = '0001'O
. . MM_MS_Identity
. . . (IEI8)iei[8] = '00010111'B
. . . (Length)iel[1] = '05'O
. . . (B4)iDigit1[4] = '1111'B
. . . (B1)oddEvenInd[1] = '0'B
. . . (B3)typeOfId[3] = '100'B
. . . (OctetStringType)otherDigits[-1] = '12345678'O
. . (FollowOnProceed)followOnProceed[8] = '10100001'B
. . (CTSPerm)cTSPerm[8] = '10100010'B
. . PLMN_List
- Constraint:
ca_DataReq
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 00 05 02 00 f1 10 00 01 17 05 f4 12 34 56 78 a1 a2

- No.: 1017
- Timestamp: 17:17:00:774_0
- RFN: 1947
- Chip: 29952
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_GMM_IdleUpdated:lt_IdleUpdated_NMO_I LINE 15
- Message Structure:
RRC_DataInd
. (IntegerType)cellId[0] = -1
. (SS_RB_Identity)rB_Id[0] = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain[0] = 0
. (START_Value)start[0] = -
. TMSIREALLOCATIONCOMPLETE
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)mMProtocolDiscriminator[4] = '0101'B
. . (MsgType)msgType[8] = '10011011'B
- Constraint:
car_UplinkDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 00 05 9b

- No.: 1027
- Timestamp: 17:17:00:776_2
- RFN: 1947
- Chip: 35328
- Event: Start Timer
- Source: ts_RRC_Delay LINE 1
- Message Structure:
no details available
- Constraint:
t_Dly (1000 Ms)
- BinaryMessage:

- No.: 1031
- Timestamp: 17:17:01:769_0
- RFN: 2047
- Chip: 9216
- Event: Timeout
- Source: ts_RRC_Delay LINE 2
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 1036
- Timestamp: 17:17:01:770_0
- RFN: 2047
- Chip: 14080
- Event: Send
- PCO: UM
- Message: RLC_UM_DATA_REQ
- Source: ts_RRC_ConnRel:lt_Send_RRC_ConnectionRelease LINE 3
- Message Structure:
RLC_UM_DATA_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 1
. uM_message
. . DL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00000000000000000000000000000000"
. . . . (IntegerType)rrc_MessageSequenceNumber[-1] = 0
. . . DL_DCCH_MessageType
. . . . RRCConnectionRelease
. . . . . r3
. . . . . . RRCConnectionRelease_r3_IEs
. . . . . . . (IntegerType)rrc_TransactionIdentifier[-1] = 0
. . . . . . . (IntegerType)n_308[-1] = 1
. . . . . . . (ReleaseCause)releaseCause[0] = 0
. . . . . . . Rplmn_Information
. . . . . . laterNonCriticalExtensions
. (BooleanType)specialLI = FALSE
- Constraint:
cas_RRC_ConnRelDCCH
- BinaryMessage:
30 10 02 01 ff 02 01 01 80 00 00 00 03 c8 00 01 01 00

- No.: 1040
- Timestamp: 17:17:01:895_0
- RFN: 2059
- Chip: 30976
- Event: Receive
- PCO: UM
- Message: RLC_UM_DATA_IND
- Source: ts_RRC_ConnRel:lt_Send_RRC_ConnectionRelease LINE 4
- Message Structure:
RLC_UM_DATA_IND
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 1
. IntegrityResult
. uM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "10101101101011101001000000111001"
. . . . (IntegerType)rrc_MessageSequenceNumber[4] = 1
. . . UL_DCCH_MessageType
. . . . RRCConnectionReleaseComplete
. . . . . (IntegerType)rrc_TransactionIdentifier[2] = 0
. . . . . FailureCauseWithProtErr
. . . . . laterNonCriticalExtensions
- Constraint:
car_RRC_ConnRelCmplUM
- BinaryMessage:
30 0e 02 01 ff 02 01 01 05 00 d6 d7 48 1c 8c 40

- No.: 1041
- Timestamp: 17:17:01:895_1
- RFN: 2059
- Chip: 32256
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ConnRel:lt_Send_RRC_ConnectionRelease LINE 4
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1044
- Timestamp: 17:17:01:896_2
- RFN: 2059
- Chip: 34304
- Event: Start Timer
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 1
- Message Structure:
no details available
- Constraint:
t_Dly (5000 Ms)
- BinaryMessage:

- No.: 1048
- Timestamp: 17:17:02:054_0
- RFN: 2075
- Chip: 30464
- Event: Receive
- PCO: UM
- Message: RLC_UM_DATA_IND
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 4
- Message Structure:
RLC_UM_DATA_IND
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 1
. IntegrityResult
. uM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00011100010101000111110101101001"
. . . . (IntegerType)rrc_MessageSequenceNumber[4] = 2
. . . UL_DCCH_MessageType
. . . . RRCConnectionReleaseComplete
. . . . . (IntegerType)rrc_TransactionIdentifier[2] = 0
. . . . . FailureCauseWithProtErr
. . . . . laterNonCriticalExtensions
- Constraint:
car_RRC_ConnRelCmplUM
- BinaryMessage:
30 0e 02 01 ff 02 01 01 05 00 8e 2a 3e b4 94 40

- No.: 1049
- Timestamp: 17:17:02:055_0
- RFN: 2075
- Chip: 32000
- Event: Cancel Timer
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 4
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 1050
- Timestamp: 17:17:02:055_1
- RFN: 2075
- Chip: 32256
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 4
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1056
- Timestamp: 17:17:02:056_1
- RFN: 2075
- Chip: 37120
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 1
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 01 0a 01 00 05 00

- No.: 1060
- Timestamp: 17:17:02:062_0
- RFN: 2076
- Chip: 22016
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 1063
- Timestamp: 17:17:02:063_1
- RFN: 2076
- Chip: 25856
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 2
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 02 0a 01 00 05 00

- No.: 1067
- Timestamp: 17:17:02:067_0
- RFN: 2077
- Chip: 2560
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 1070
- Timestamp: 17:17:02:068_0
- RFN: 2077
- Chip: 6400
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 3
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 03 0a 01 00 05 00

- No.: 1074
- Timestamp: 17:17:02:073_0
- RFN: 2077
- Chip: 25856
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 3
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 1077
- Timestamp: 17:17:02:074_0
- RFN: 2077
- Chip: 30208
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 4
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 04 0a 01 00 05 00

- No.: 1081
- Timestamp: 17:17:02:080_0
- RFN: 2078
- Chip: 14592
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 4
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 1084
- Timestamp: 17:17:02:082_0
- RFN: 2078
- Chip: 22272
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 1
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 136
. . . . . UL_RLC_Mode
. . . . . . UL_UM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (NoExplicitDiscard)timerBasedNoExplicit[0] = 9
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 1
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 1
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_UM_Info
- BinaryMessage:
30 22 02 01 ff 02 01 01 0a 01 00 30 17 30 0d 05 00 30 09 02 02 00 88 30 03 0a 01 09 30 06 02 01 01 02 01 01

- No.: 1088
- Timestamp: 17:17:02:086_0
- RFN: 2078
- Chip: 37888
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 1089
- Timestamp: 17:17:02:088_0
- RFN: 2079
- Chip: 5888
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 3
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 2
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 2
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 2
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 02 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 13 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 02 02 01 02

- No.: 1093
- Timestamp: 17:17:02:096_0
- RFN: 2079
- Chip: 37888
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 4
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 1094
- Timestamp: 17:17:02:098_0
- RFN: 2080
- Chip: 5888
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 5
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 3
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 3
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 3
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 03 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 13 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 03 02 01 03

- No.: 1098
- Timestamp: 17:17:02:106_0
- RFN: 2080
- Chip: 38144
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 6
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 3
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 1099
- Timestamp: 17:17:02:108_0
- RFN: 2081
- Chip: 6656
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 7
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 4
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 4
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 4
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 04 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 13 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 04 02 01 04

- No.: 1103
- Timestamp: 17:17:02:117_0
- RFN: 2082
- Chip: 1280
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 8
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 4
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 1126
- Timestamp: 17:17:02:119_6
- RFN: 2082
- Chip: 12288
- Event: Start Timer
- Source: ts_GMM_IdleUpdated:lt_IdleUpdated_NMO_I LINE 17
- Message Structure:
no details available
- Constraint:
t_WaitS (1 Sec)
- BinaryMessage:

- No.: 1133
- Timestamp: 17:17:03:118_0
- RFN: 2182
- Chip: 7168
- Event: Timeout
- Source: ts_GMM_IdleUpdated:lt_IdleUpdated_NMO_I LINE 18
- Message Structure:
no details available
- Constraint:
t_WaitS
- BinaryMessage:

- No.: 1135
- Timestamp: 17:17:03:118_2
- RFN: 2182
- Chip: 8192
- Event: Start Timer
- Source: ts_GMM_IdleUpdated:lt_IdleUpdated_NMO_I LINE 19
- Message Structure:
no details available
- Constraint:
t_WaitS (60 Sec)
- BinaryMessage:

- No.: 1137
- Timestamp: 17:17:03:128_0
- RFN: 2183
- Chip: 9728
- Event: Send
- PCO: Ut
- Message: AT_CmdReq
- Source: ts_AT_TriggerGMM_Attach LINE 1
- Message Structure:
AT_CmdReq
. (IA5StringType)cmd[-1] = "AT+CGATT=1"
. (HexStringType)sMS_BlockMode[-1] = -
- Constraint:
ca_AT_CmdReq
- BinaryMessage:
41 54 2b 43 47 41 54 54 3d 31 3c 43 52 3e

- No.: 1141
- Timestamp: 17:17:04:238_0
- RFN: 2294
- Chip: 7424
- Event: Receive
- PCO: Ut
- Message: AT_CmdCnf
- Source: ts_AT_TriggerGMM_Attach LINE 2
- Message Structure:
AT_CmdCnf
. (BooleanType)result = TRUE
. (IA5StringType)resultString[18] = "OK"
. (HexStringType)sMS_BlockMode[0] = -
- Constraint:
ca_AT_CmdCnf
- BinaryMessage:
80 3c 43 52 3e 3c 4c 46 3e 4f 4b 3c 43 52 3e 3c 4c 46 3e

- No.: 1158
- Timestamp: 17:17:04:241_0
- RFN: 2294
- Chip: 16640
- Event: Receive
- PCO: CPHY
- Message: CPHY_Out_of_Sync_IND
- Source: RRC_DefConnEst LINE 7
- Message Structure:
CPHY_Out_of_Sync_IND
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 20
- Constraint:
ca_OutOfSyncInd
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 1159
- Timestamp: 17:17:04:241_1
- RFN: 2294
- Chip: 17664
- Event: Cancel Timer
- Source: RRC_DefConnEst LINE 7
- Message Structure:
no details available
- Constraint:
t_T312
- BinaryMessage:

- No.: 1160
- Timestamp: 17:17:04:241_2
- RFN: 2294
- Chip: 18176
- Event: Default
- Source: RRC_DefConnEst LINE 0
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1161
- Timestamp: 17:17:04:241_3
- RFN: 2294
- Chip: 18432
- Event: Default
- Source: ts_RRC_ConnEst:lt_RcvConnReq LINE 2
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1166
- Timestamp: 17:17:06:492_0
- RFN: 2519
- Chip: 23296
- Event: Receive
- PCO: TM
- Message: RLC_TR_DATA_IND
- Source: ts_RRC_ConnEst:lt_RcvConnReq LINE 2
- Message Structure:
RLC_TR_DATA_IND
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 0
. tM_message
. . UL_CCCH_Message
. . . IntegrityCheckInfo
. . . UL_CCCH_MessageType
. . . . RRCConnectionRequest
. . . . . InitialUE_Identity
. . . . . . TMSI_and_LAI_GSM_MAP
. . . . . . . (BitStringType)tmsi[32] = "00010010001101000101011001111000"
. . . . . . . LAI
. . . . . . . . PLMN_Identity
. . . . . . . . . MCC
. . . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . . (IntegerType)_elem[4] = 1
. . . . . . . . . MNC
. . . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . . (IntegerType)_elem[4] = 1
. . . . . . . . (BitStringType)lac[16] = '0000000000000001'B
. . . . . (EstablishmentCause)establishmentCause[5] = 12
. . . . . (ProtocolErrorIndicator)protocolErrorIndicator[1] = 0
. . . . . MeasuredResultsOnRACH
. . . . . v3d0NonCriticalExtensions
- Constraint:
car_RRC_ConnReq
- BinaryMessage:
30 11 02 01 00 02 01 00 21 12 34 56 78 00 10 08 00 0b 00

- No.: 1170
- Timestamp: 17:17:06:501_0
- RFN: 2520
- Chip: 20736
- Event: Send
- PCO: UM
- Message: RLC_UM_DATA_REQ
- Source: ts_RRC_ConnEst:lt_Send_ConnSetUp LINE 22
- Message Structure:
RLC_UM_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 0
. uM_message
. . DL_CCCH_Message
. . . IntegrityCheckInfo
. . . DL_CCCH_MessageType
. . . . RRCConnectionSetup
. . . . . r3
. . . . . . RRCConnectionSetup_r3_IEs
. . . . . . . InitialUE_Identity
. . . . . . . . TMSI_and_LAI_GSM_MAP
. . . . . . . . . (BitStringType)tmsi[32] = "00010010001101000101011001111000"
. . . . . . . . . LAI
. . . . . . . . . . PLMN_Identity
. . . . . . . . . . . MCC
. . . . . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . . . . (IntegerType)_elem[4] = 1
. . . . . . . . . . . MNC
. . . . . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . . . . (IntegerType)_elem[4] = 1
. . . . . . . . . . (BitStringType)lac[16] = '0000000000000001'B
. . . . . . . (IntegerType)rrc_TransactionIdentifier[-1] = 0
. . . . . . . (IntegerType)activationTime[-1] = -
. . . . . . . U_RNTI
. . . . . . . . (BitStringType)srnc_Identity[12] = "000000000001"
. . . . . . . . (BitStringType)s_RNTI[20] = "00000000000000000001"
. . . . . . . (BitStringType)new_c_RNTI[16] = -
. . . . . . . (RRC_StateIndicator)rrc_StateIndicator[0] = 0
. . . . . . . (IntegerType)utran_DRX_CycleLengthCoeff[-1] = 9
. . . . . . . CapabilityUpdateRequirement
. . . . . . . . (BooleanType)ue_RadioCapabilityFDDUpdateRequirement = TRUE
. . . . . . . . (BooleanType)ue_RadioCapabilityTDDUpdateRequirement = FALSE
. . . . . . . . SystemSpecificCapUpdateReqList
. . . . . . . . . (SystemSpecificCapUpdateReq)_elem[0] = 0
. . . . . . . SRB_InformationSetupList2
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity[-1] = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_UM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 1
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex[-1] = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 1
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity[-1] = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 2
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 2
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 2
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 2
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex[-1] = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 2
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 2
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity[-1] = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 3
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 3
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 3
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 3
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex[-1] = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 3
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 3
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity[-1] = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 4
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 4
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 4
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 4
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex[-1] = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 4
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 4
. . . . . . . UL_CommonTransChInfo
. . . . . . . . TFC_Subset
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . TFCS
. . . . . . . . . . . ExplicitTFCS_Configuration
. . . . . . . . . . . . TFCS_ReconfAdd
. . . . . . . . . . . . . ctfcSize
. . . . . . . . . . . . . . ctfc2Bit
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . . . . . . . (IntegerType)ctfc2[-1] = 0
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . . . . . . . (IntegerType)ctfc2[-1] = 1
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC[-1] = 11
. . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaD[-1] = 15
. . . . . . . . . . . . . . . . . . . (IntegerType)referenceTFC_ID[-1] = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . UL_AddReconfTransChInfoList
. . . . . . . . UL_AddReconfTransChInformation
. . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType[0] = 0
. . . . . . . . . (IntegerType)transportChannelIdentity[-1] = 5
. . . . . . . . . TransportFormatSet
. . . . . . . . . . DedicatedTransChTFS
. . . . . . . . . . . tti
. . . . . . . . . . . . DedicatedDynamicTF_InfoList
. . . . . . . . . . . . . DedicatedDynamicTF_Info
. . . . . . . . . . . . . . rlc_Size
. . . . . . . . . . . . . . . BitModeRLC_SizeInfo
. . . . . . . . . . . . . . . . sizeType2
. . . . . . . . . . . . . . . . . (IntegerType)part1[-1] = 2
. . . . . . . . . . . . . . . . . (IntegerType)part2[-1] = -
. . . . . . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . LogicalChannelList
. . . . . . . . . . . SemistaticTF_Information
. . . . . . . . . . . . ChannelCodingType
. . . . . . . . . . . . . (CodingRate)convolutional[0] = 1
. . . . . . . . . . . . (IntegerType)rateMatchingAttribute[-1] = 192
. . . . . . . . . . . . (CRC_Size)crc_Size[0] = 3
. . . . . . . DL_CommonTransChInfo
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . dl_Parameters
. . . . . . . DL_AddReconfTransChInfoList
. . . . . . . . DL_AddReconfTransChInformation
. . . . . . . . . (DL_TrCH_Type)dl_TransportChannelType[0] = 0
. . . . . . . . . (IntegerType)dl_transportChannelIdentity[-1] = 10
. . . . . . . . . tfs_SignallingMode
. . . . . . . . . . UL_TransportChannelIdentity
. . . . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType[0] = 0
. . . . . . . . . . . (IntegerType)ul_TransportChannelIdentity[-1] = 5
. . . . . . . . . QualityTarget
. . . . . . . . . . (IntegerType)bler_QualityValue[-1] = -20
. . . . . . . . . TM_SignallingInfo
. . . . . . . FrequencyInfo
. . . . . . . (IntegerType)maxAllowedUL_TX_Power[-1] = -
. . . . . . . UL_ChannelRequirement
. . . . . . . . UL_DPCH_Info
. . . . . . . . . UL_DPCH_PowerControlInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (IntegerType)dpcch_PowerOffset[-1] = -40
. . . . . . . . . . . (IntegerType)pc_Preamble[-1] = 1
. . . . . . . . . . . (IntegerType)sRB_delay[-1] = 7
. . . . . . . . . . . PowerControlAlgorithm
. . . . . . . . . . . . (IntegerType)algorithm1[-1] = 1
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (ScramblingCodeType)scramblingCodeType[0] = 1
. . . . . . . . . . . (IntegerType)scramblingCode[-1] = 0
. . . . . . . . . . . (IntegerType)numberOfDPDCH[-1] = -
. . . . . . . . . . . (SpreadingFactor)spreadingFactor[0] = 4
. . . . . . . . . . . (BooleanType)tfci_Existence = TRUE
. . . . . . . . . . . (IntegerType)numberOfFBI_Bits[-1] = -
. . . . . . . . . . . (PuncturingLimit)puncturingLimit[0] = 15
. . . . . . . DL_CommonInformation
. . . . . . . . DL_DPCH_InfoCommon
. . . . . . . . . cfnHandling
. . . . . . . . . . initialise
. . . . . . . . . . . (IntegerType)cfntargetsfnframeoffset[-1] = -
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . DL_DPCH_PowerControlInfo
. . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . (DPC_Mode)dpc_Mode[0] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPilot_pdpdch[-1] = 0
. . . . . . . . . . . Dl_rate_matching_restriction
. . . . . . . . . . . SF512_AndPilot
. . . . . . . . . . . . (PilotBits128)sfd128[0] = 0
. . . . . . . . . . . (PositionFixedOrFlexible)positionFixedOrFlexible[0] = 0
. . . . . . . . . . . (BooleanType)tfci_Existence = FALSE
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . (IntegerType)defaultDPCH_OffsetValue[-1] = 459
. . . . . . . . . . DPCH_CompressedModeInfo
. . . . . . . . . . (TX_DiversityMode)tx_DiversityMode[0] = 0
. . . . . . . . . . SSDT_Information
. . . . . . . DL_InformationPerRL_List
. . . . . . . . DL_InformationPerRL
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . PrimaryCPICH_Info
. . . . . . . . . . . . (IntegerType)primaryScramblingCode[-1] = 100
. . . . . . . . . . . PDSCH_SHO_DCH_Info
. . . . . . . . . . . PDSCH_CodeMapping
. . . . . . . . . DL_DPCH_InfoPerRL
. . . . . . . . . . fdd
. . . . . . . . . . . (PCPICH_UsageForChannelEst)pCPICH_UsageForChannelEst[0] = 0
. . . . . . . . . . . (IntegerType)dpch_FrameOffset[-1] = 18
. . . . . . . . . . . SecondaryCPICH_Info
. . . . . . . . . . . DL_ChannelisationCodeList
. . . . . . . . . . . . DL_ChannelisationCode
. . . . . . . . . . . . . (IntegerType)secondaryScramblingCode[-1] = 1
. . . . . . . . . . . . . SF512_AndCodeNumber
. . . . . . . . . . . . . . (IntegerType)sf128[-1] = 0
. . . . . . . . . . . . . (ScramblingCodeChange)scramblingCodeChange[0] = 1
. . . . . . . . . . . (IntegerType)tpc_CombinationIndex[-1] = 0
. . . . . . . . . . . (SSDT_CellIdentity)ssdt_CellIdentity[0] = -
. . . . . . . . . . . (ClosedLoopTimingAdjMode)closedLoopTimingAdjMode[0] = -
. . . . . . . . . SCCPCH_InfoForFACH
. . . . . . laterNonCriticalExtensions
. (BooleanType)specialLI = TRUE
- Constraint:
cas_RRC_ConnSetup
- BinaryMessage:
30 78 02 01 00 02 01 00 30 e7 22 46 8a cf 00 02 01 00 01 00 04 00 00 4d 82 69 3a 10 10 89 0d 42 00 02 81 9e 8e 46 c9 a6 7c 9c 4e 74 20 a5 12 3a 8c 00 15 13 3d 1c 8d 93 4c f9 38 9c e8 42 52 24 b5 28 00 4a 46 7a 39 1b 26 99 f2 71 39 d0 86 b4 49 ea 70 00 d4 c8 00 06 25 2b f0 02 00 08 82 23 bf 66 08 98 95 a5 47 a2 00 00 01 3f 90 0a 14 e5 82 06 40 09 0c 28 08 01 01 ff

- No.: 1191
- Timestamp: 17:17:06:524_1
- RFN: 2522
- Chip: 30464
- Event: Start Timer
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 3
- Message Structure:
no details available
- Constraint:
t_WaitMS (13500 Ms)
- BinaryMessage:

- No.: 1198
- Timestamp: 17:17:06:723_1
- RFN: 2542
- Chip: 28160
- Event: Receive
- PCO: CPHY
- Message: CPHY_Sync_IND
- Source: RRC_DefConnEst LINE 5
- Message Structure:
CPHY_Sync_IND
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 20
- Constraint:
ca_SyncInd
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 1199
- Timestamp: 17:17:06:724_0
- RFN: 2542
- Chip: 28928
- Event: Cancel Timer
- Source: RRC_DefConnEst LINE 5
- Message Structure:
no details available
- Constraint:
t_T312
- BinaryMessage:

- No.: 1200
- Timestamp: 17:17:06:724_1
- RFN: 2542
- Chip: 29440
- Event: Default
- Source: RRC_DefConnEst LINE 0
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1201
- Timestamp: 17:17:06:724_2
- RFN: 2542
- Chip: 29952
- Event: Default
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1208
- Timestamp: 17:17:06:825_0
- RFN: 2552
- Chip: 34816
- Event: Receive
- PCO: AM
- Message: RLC_AM_DATA_IND
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
RLC_AM_DATA_IND
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 2
. IntegrityResult
. . (IntegrityStatus)integrityUsed[0] = 4294967296
. aM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . UL_DCCH_MessageType
. . . . RRCConnectionSetupComplete
. . . . . (IntegerType)rrc_TransactionIdentifier[2] = 0
. . . . . STARTList
. . . . . . STARTSingle
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity[1] = 1
. . . . . . . (BitStringType)start_Value[20] = "00000000000000000010"
. . . . . . STARTSingle
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity[1] = 0
. . . . . . . (BitStringType)start_Value[20] = "00000000000000000010"
. . . . . UE_RadioAccessCapability
. . . . . . (AccessStratumReleaseIndicator)accessStratumReleaseIndicator[0] = 0
. . . . . . PDCP_Capability
. . . . . . . (BooleanType)losslessSRNS_RelocationSupport = FALSE
. . . . . . . supportForRfc2507
. . . . . . . . (MaxHcContextSpace)supported[3] = 4
. . . . . . RLC_Capability
. . . . . . . (TotalRLC_AM_BufferSize)totalRLC_AM_BufferSize[3] = 2
. . . . . . . (MaximumRLC_WindowSize)maximumRLC_WindowSize[1] = 0
. . . . . . . (MaximumAM_EntityNumberRLC_Cap)maximumAM_EntityNumber[3] = 3
. . . . . . TransportChannelCapability
. . . . . . . DL_TransChCapability
. . . . . . . . (MaxNoBits)maxNoBitsReceived[4] = 7
. . . . . . . . (MaxNoBits)maxConvCodeBitsReceived[4] = 1
. . . . . . . . TurboSupport
. . . . . . . . . (MaxNoBits)supported[4] = 7
. . . . . . . . (MaxSimultaneousTransChsDL)maxSimultaneousTransChs[2] = 1
. . . . . . . . (IntegerType)maxSimultaneousCCTrCH_Count[3] = 1
. . . . . . . . (MaxTransportBlocksDL)maxReceivedTransportBlocks[4] = 3
. . . . . . . . (MaxNumberOfTFC_DL)maxNumberOfTFC[4] = 5
. . . . . . . . (MaxNumberOfTF)maxNumberOfTF[3] = 1
. . . . . . . UL_TransChCapability
. . . . . . . . (MaxNoBits)maxNoBitsTransmitted[4] = 3
. . . . . . . . (MaxNoBits)maxConvCodeBitsTransmitted[4] = 1
. . . . . . . . TurboSupport
. . . . . . . . . (MaxNoBits)supported[4] = 3
. . . . . . . . (MaxSimultaneousTransChsUL)maxSimultaneousTransChs[3] = 2
. . . . . . . . modeSpecificInfo
. . . . . . . . (MaxTransportBlocksUL)maxTransmittedBlocks[4] = 4
. . . . . . . . (MaxNumberOfTFC_UL)maxNumberOfTFC[4] = 5
. . . . . . . . (MaxNumberOfTF)maxNumberOfTF[3] = 0
. . . . . . RF_Capability
. . . . . . . fddRF_Capability
. . . . . . . . (IntegerType)ue_PowerClass[2] = 4
. . . . . . . . (TxRxFrequencySeparation)txRxFrequencySeparation[2] = 0
. . . . . . . tddRF_Capability
. . . . . . PhysicalChannelCapability
. . . . . . . fddPhysChCapability
. . . . . . . . DL_PhysChCapabilityFDD
. . . . . . . . . (IntegerType)maxNoDPCH_PDSCH_Codes[3] = 1
. . . . . . . . . (MaxNoPhysChBitsReceived)maxNoPhysChBitsReceived[4] = 6
. . . . . . . . . (BooleanType)supportForSF_512 = FALSE
. . . . . . . . . (BooleanType)supportOfPDSCH = FALSE
. . . . . . . . . SimultaneousSCCPCH_DPCH_Reception
. . . . . . . . UL_PhysChCapabilityFDD
. . . . . . . . . (MaxNoDPDCH_BitsTransmitted)maxNoDPDCH_BitsTransmitted[4] = 3
. . . . . . . . . (BooleanType)supportOfPCPCH = FALSE
. . . . . . . tddPhysChCapability
. . . . . . UE_MultiModeRAT_Capability
. . . . . . . MultiRAT_Capability
. . . . . . . . (BooleanType)supportOfGSM = FALSE
. . . . . . . . (BooleanType)supportOfMulticarrier = FALSE
. . . . . . . (MultiModeCapability)multiModeCapability[2] = 1
. . . . . . SecurityCapability
. . . . . . . (BitStringType)cipheringAlgorithmCap[16] = '0000000000000011'B
. . . . . . . (BitStringType)integrityProtectionAlgorithmCap[16] = '0000000000000010'B
. . . . . . UE_Positioning_Capability
. . . . . . . (BooleanType)standaloneLocMethodsSupported = FALSE
. . . . . . . (BooleanType)ue_BasedOTDOA_Supported = FALSE
. . . . . . . (NetworkAssistedGPS_Supported)networkAssistedGPS_Supported[2] = 3
. . . . . . . (BooleanType)supportForUE_GPS_TimingOfCellFrames = FALSE
. . . . . . . (BooleanType)supportForIPDL = FALSE
. . . . . . MeasurementCapability
. . . . . . . CompressedModeMeasCapability
. . . . . . . . (BooleanType)fdd_Measurements = TRUE
. . . . . . . . (BooleanType)tdd_Measurements = -
. . . . . . . . GSM_Measurements
. . . . . . . . . (BooleanType)gsm900 = TRUE
. . . . . . . . . (BooleanType)dcs1800 = TRUE
. . . . . . . . . (BooleanType)gsm1900 = TRUE
. . . . . . . . (BooleanType)multiCarrierMeasurements = FALSE
. . . . . . . CompressedModeMeasCapability
. . . . . . . . (BooleanType)fdd_Measurements = TRUE
. . . . . . . . (BooleanType)tdd_Measurements = -
. . . . . . . . GSM_Measurements
. . . . . . . . . (BooleanType)gsm900 = TRUE
. . . . . . . . . (BooleanType)dcs1800 = TRUE
. . . . . . . . . (BooleanType)gsm1900 = TRUE
. . . . . . . . (BooleanType)multiCarrierMeasurements = FALSE
. . . . . v370NonCriticalExtensions
- Constraint:
car_RRC_ConnSetupCmpl
- BinaryMessage:
30 27 02 01 ff 02 01 02 0a 05 01 00 00 00 00 4a 0c 00 00 80 00 05 62 37 1b a0 d4 98 cd 11 45 90 60 61 00 03 00 02 31 f9 f8

- No.: 1209
- Timestamp: 17:17:06:827_0
- RFN: 2553
- Chip: 3328
- Event: Cancel Timer
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
t_WaitMS
- BinaryMessage:

- No.: 1210
- Timestamp: 17:17:06:827_1
- RFN: 2553
- Chip: 3584
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1228
- Timestamp: 17:17:06:854_0
- RFN: 2555
- Chip: 32768
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_GMM_IdleUpdated:lt_IdleUpdated_NMO_I LINE 22
- Message Structure:
RRC_DataInd
. (IntegerType)cellId[0] = -1
. (SS_RB_Identity)rB_Id[0] = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain[0] = 1
. (START_Value)start[20] = '00000000000000000010'B
. ATTACHREQUEST
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)gMMProtocolDiscriminator[4] = '1000'B
. . (MsgType)msgType[8] = '00000001'B
. . MS_NetworkCap_lv
. . . (Length)iel[1] = '02'O
. . . (OctetStringType)value[2] = 'E540'O
. . CiphKeySeqNum
. . . (B1)spare1[1] = '0'B
. . . (KeySeq)keySeq[3] = '111'B
. . AttachType
. . . (B1)pre_for[1] = '0'B
. . . (B3)type[3] = '011'B
. . DRXparamter
. . . (B8)splitPGcycleCode[8] = '00000111'B
. . . (B4)cnDRXcoef[4] = '0000'B
. . . (B1)splitOnCCCH[1] = '0'B
. . . (B3)nonDRXtimer[3] = '100'B
. . MS_Identity_lv
. . . (Length)iel[1] = '08'O
. . . (B4)iDigit1[4] = '0000'B
. . . (B1)oddEvenInd[1] = '1'B
. . . (B3)typeOfId[3] = '001'B
. . . (OctetStringType)otherDigits[7] = '10101032540636'O
. . RAI_v
. . . (OctetStringType)plmn[3] = '00F110'O
. . . (OctetStringType)lac[2] = 'FFFE'O
. . . (OctetStringType)rac[1] = '05'O
. . MSRadioAccessCap_lv
. . . (Length)iel[1] = '0B'O
. . . (OctetStringType)value[11] = '15F38233542A332644A198'O
. . PTMSI_Signature
. . GPRS_Timer
. . . (IEI8)iei[8] = '00010111'B
. . . (B3)unit[3] = '000'B
. . . (B5)value[5] = '10110'B
. . TMSI_Status
- Constraint:
car_PS_InitDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 03 04 04 00 00 20 08 01 02 e5 40 73 07 04 08 09 10 10 10 32 54 06 36 00 f1 10 ff fe 05 0b 15 f3 82 33 54 2a 33 26 44 a1 98 17 16

- No.: 1229
- Timestamp: 17:17:06:855_0
- RFN: 2555
- Chip: 35584
- Event: Cancel Timer
- Source: ts_GMM_IdleUpdated:lt_IdleUpdated_NMO_I LINE 22
- Message Structure:
no details available
- Constraint:
t_WaitS
- BinaryMessage:

- No.: 1265
- Timestamp: 17:17:06:861_0
- RFN: 2556
- Chip: 18688
- Event: Send
- PCO: Dc
- Message: RRC_DataReq
- Source: ts_GMM_Authentication LINE 2
- Message Structure:
RRC_DataReq
. (IntegerType)cellId[-1] = -1
. (SS_RB_Identity)rB_Id[-1] = 3
. (LogicChGERAN)ch[-1] = -
. (SapId)sapId[1] = -
. (SS_CN_DomainIdentity)cN_Domain[-1] = 1
. AUTHENTICATIONANDCIPHERINGREQUEST
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)gMMProtocolDiscriminator[4] = '1000'B
. . (MsgType)msgType[8] = '00010010'B
. . IMEISVRequest
. . . (B1)spare1[1] = '0'B
. . . (B3)value[3] = '000'B
. . CiphAlgorithm
. . . (B1)spare1[1] = '0'B
. . . (B3)algorithm[3] = '001'B
. . AC_ReferenceNumber
. . . (B4)value[4] = '0011'B
. . ForceToStandby
. . . (B1)spare[1] = '0'B
. . . (B3)value[3] = '000'B
. . AuthenticationParamterRAND
. . . (IEI8)iei[8] = '00100001'B
. . . (BitStringType)randValue[128] = '01010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101'B
. . CiphKeySeqNum_tv
. . . (IEI4)iei[4] = '1000'B
. . . (B1)spare1[1] = '0'B
. . . (KeySeq)keySeq[3] = '000'B
. . GMM_AUTN
. . . (IEI8)iei[8] = '00101000'B
. . . (Length)iel[1] = '10'O
. . . (BitStringType)aUTN[128] = '01010110010100010101000001010011010100100101110100000000000000000101010101010100010101110101011001010001010100000101001101010010'B
- Constraint:
ca_PS_DataReq
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 08 12 01 30 21 55 55 55 55 55 55 55 55 55 55 55 55 55 55 55 55 80 28 10 56 51 50 53 52 5d 00 00 55 54 57 56 51 50 53 52

- No.: 1269
- Timestamp: 17:17:07:134_0
- RFN: 2583
- Chip: 30720
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_GMM_Authentication LINE 3
- Message Structure:
RRC_DataInd
. (IntegerType)cellId[0] = -1
. (SS_RB_Identity)rB_Id[0] = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain[0] = 1
. (START_Value)start[0] = -
. AUTHENTICATIONANDCIPHERINGRESPONSE
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)gMMProtocolDiscriminator[4] = '1000'B
. . (MsgType)msgType[8] = '00010011'B
. . (B4)spare4[4] = '0000'B
. . AC_ReferenceNumber
. . . (B4)value[4] = '0011'B
. . AuthRsp_tv
. . . (IEI8)iei[8] = '00100010'B
. . . (BitStringType)value[32] = '01010101010101000101011101010110'B
. . GMM_MS_Identity
. . AuthRspExt
. . . (IEI8)iei[8] = '00101001'B
. . . (Length)iel[1] = '0C'O
. . . (BitStringType)rES[96] = '010100010101000001010011010100100101110101011100010111110101111001011001010110000101101101011010'B
- Constraint:
car_PS_UplinkDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 08 13 03 22 55 54 57 56 29 0c 51 50 53 52 5d 5c 5f 5e 59 58 5b 5a

- No.: 1272
- Timestamp: 17:17:07:135_0
- RFN: 2583
- Chip: 33792
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_GMM_Authentication LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1313
- Timestamp: 17:17:07:140_0
- RFN: 2584
- Chip: 16128
- Event: Send
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_REQ
- Source: ts_SS_DownloadSecurityKey:lt_DownloadKeyCRLC LINE 1
- Message Structure:
CRLC_SecurityMode_Config_REQ
. (IntegerType)cellId[-1] = -1
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity[0] = 1
. . (BitStringType)startValue[20] = "00000000000000000000"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = '01010111010101100101000101010000010100110101001001011101010111000101111101011110010110010101100001011011010110100101010101010100'B
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CRLC_SecurityModeCfgReq
- BinaryMessage:
30 21 02 01 ff 30 1c 0a 01 01 03 04 04 00 00 00 03 11 00 57 56 51 50 53 52 5d 5c 5f 5e 59 58 5b 5a 55 54

- No.: 1314
- Timestamp: 17:17:07:140_1
- RFN: 2584
- Chip: 17920
- Event: Receive
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_CNF
- Source: ts_SS_DownloadSecurityKey:lt_DownloadKeyCRLC LINE 2
- Message Structure:
CRLC_SecurityMode_Config_CNF
. (IntegerType)cellId[0] = -1
- Constraint:
ca_CRLC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1321
- Timestamp: 17:17:07:141_6
- RFN: 2584
- Chip: 22272
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 1
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 0
. (IntegerType)count_I_LSB_UL[-1] = -
. (IntegerType)count_I_LSB_DL[-1] = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 00 02 01 00 02 01 00

- No.: 1322
- Timestamp: 17:17:07:142_0
- RFN: 2584
- Chip: 23808
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 2
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 0
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 00 02 01 00

- No.: 1323
- Timestamp: 17:17:07:142_1
- RFN: 2584
- Chip: 25600
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 3
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 1
. (IntegerType)count_I_LSB_UL[-1] = -
. (IntegerType)count_I_LSB_DL[-1] = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 01 02 01 00

- No.: 1324
- Timestamp: 17:17:07:143_0
- RFN: 2584
- Chip: 27136
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 4
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 1
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 1325
- Timestamp: 17:17:07:143_1
- RFN: 2584
- Chip: 28928
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 5
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 2
. (IntegerType)count_I_LSB_UL[-1] = -
. (IntegerType)count_I_LSB_DL[-1] = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 02 02 01 00

- No.: 1326
- Timestamp: 17:17:07:144_0
- RFN: 2584
- Chip: 30720
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 6
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 2
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 1327
- Timestamp: 17:17:07:144_1
- RFN: 2584
- Chip: 32256
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 7
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 3
. (IntegerType)count_I_LSB_UL[-1] = -
. (IntegerType)count_I_LSB_DL[-1] = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 03 02 01 00

- No.: 1328
- Timestamp: 17:17:07:145_0
- RFN: 2584
- Chip: 33792
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 8
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 3
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 1329
- Timestamp: 17:17:07:145_1
- RFN: 2584
- Chip: 35840
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 9
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 4
. (IntegerType)count_I_LSB_UL[-1] = -
. (IntegerType)count_I_LSB_DL[-1] = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 04 02 01 00

- No.: 1330
- Timestamp: 17:17:07:145_2
- RFN: 2584
- Chip: 37376
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 10
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 4
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 1334
- Timestamp: 17:17:07:146_3
- RFN: 2585
- Chip: 3072
- Event: Send
- PCO: CRLC
- Message: CRLC_Integrity_Activate_REQ
- Source: ts_CRLC_DL_Integrity LINE 1
- Message Structure:
CRLC_Integrity_Activate_REQ
. (IntegerType)cellId[-1] = -1
. (CN_DomainIdentity)cn_DomainIdentity[0] = 1
. IntegrityActivationInfo
. . IntegrityProtectionModeInfo
. . . IntegrityProtectionModeCommand
. . . . startIntegrityProtection
. . . . . (BitStringType)integrityProtInitNumber[32] = "00000000000000000000000000000001"
. . . (IntegrityProtectionAlgorithm)integrityProtectionAlgorithm[0] = 0
- Constraint:
ca_CRLC_DL_IntegrityActivateReq
- BinaryMessage:
30 14 02 01 ff 0a 01 01 30 0c 30 07 03 05 00 00 00 00 01 0a 01 00

- No.: 1335
- Timestamp: 17:17:07:147_0
- RFN: 2585
- Chip: 4864
- Event: Receive
- PCO: CRLC
- Message: CRLC_Integrity_Activate_CNF
- Source: ts_CRLC_DL_Integrity LINE 2
- Message Structure:
CRLC_Integrity_Activate_CNF
. (IntegerType)cellId[0] = -1
- Constraint:
ca_CRLC_IntegrityActivateCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1342
- Timestamp: 17:17:07:148_3
- RFN: 2585
- Chip: 9984
- Event: Send
- PCO: CRLC
- Message: CRLC_Integrity_Activate_REQ
- Source: ts_RB2_UL_IntegrityActivate LINE 1
- Message Structure:
CRLC_Integrity_Activate_REQ
. (IntegerType)cellId[-1] = -1
. (CN_DomainIdentity)cn_DomainIdentity[0] = 1
. IntegrityActivationInfo
. . IntegrityProtActivationInfoList
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity[-1] = 2
. . . . (IntegerType)rrc_MessageSequenceNumber[-1] = 0
- Constraint:
ca_CRLC_UL_IntegrityActivateReq
- BinaryMessage:
30 10 02 01 ff 0a 01 01 30 08 30 06 02 01 02 02 01 00

- No.: 1343
- Timestamp: 17:17:07:149_0
- RFN: 2585
- Chip: 13312
- Event: Receive
- PCO: CRLC
- Message: CRLC_Integrity_Activate_CNF
- Source: ts_RB2_UL_IntegrityActivate LINE 2
- Message Structure:
CRLC_Integrity_Activate_CNF
. (IntegerType)cellId[0] = -1
- Constraint:
ca_CRLC_IntegrityActivateCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1350
- Timestamp: 17:17:07:151_0
- RFN: 2585
- Chip: 19968
- Event: Send
- PCO: AM
- Message: RLC_AM_DATA_REQ
- Source: ts_RRC_Security:lt_SendSecurityModeCommand LINE 16
- Message Structure:
RLC_AM_DATA_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 2
. AmConfirmationRequest
. aM_message
. . DL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00000000000000000000000000000000"
. . . . (IntegerType)rrc_MessageSequenceNumber[-1] = 0
. . . DL_DCCH_MessageType
. . . . SecurityModeCommand
. . . . . r3
. . . . . . SecurityModeCommand_r3_IEs
. . . . . . . (IntegerType)rrc_TransactionIdentifier[-1] = 0
. . . . . . . SecurityCapability
. . . . . . . . (BitStringType)cipheringAlgorithmCap[16] = '0000000000000011'B
. . . . . . . . (BitStringType)integrityProtectionAlgorithmCap[16] = '0000000000000010'B
. . . . . . . CipheringModeInfo
. . . . . . . IntegrityProtectionModeInfo
. . . . . . . . IntegrityProtectionModeCommand
. . . . . . . . . startIntegrityProtection
. . . . . . . . . . (BitStringType)integrityProtInitNumber[32] = "00000000000000000000000000000001"
. . . . . . . . (IntegrityProtectionAlgorithm)integrityProtectionAlgorithm[0] = 0
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity[0] = 1
. . . . . . . InterRAT_UE_SecurityCapList
. . . . . . laterNonCriticalExtensions
- Constraint:
cas_RRC_SecModeCmd
- BinaryMessage:
30 17 02 01 ff 02 01 02 05 00 80 00 00 00 04 04 00 01 80 01 40 00 00 00 30

- No.: 1359
- Timestamp: 17:17:07:275_0
- RFN: 2597
- Chip: 31488
- Event: Receive
- PCO: AM
- Message: RLC_AM_DATA_IND
- Source: ts_RRC_Security:lt_StartSecurity_UE LINE 8
- Message Structure:
RLC_AM_DATA_IND
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 2
. IntegrityResult
. . (IntegrityStatus)integrityUsed[0] = 0
. aM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "10000001100000001110110111011101"
. . . . (IntegerType)rrc_MessageSequenceNumber[4] = 1
. . . UL_DCCH_MessageType
. . . . SecurityModeComplete
. . . . . (IntegerType)rrc_TransactionIdentifier[2] = 0
. . . . . IntegrityProtActivationInfo
. . . . . . RRC_MessageSequenceNumberList
. . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . (IntegerType)_elem[4] = 0
. . . . . laterNonCriticalExtensions
- Constraint:
car_RRC_SecModeCmpl
- BinaryMessage:
30 12 02 01 ff 02 01 02 0a 01 00 c0 c0 76 ee 8d 21 00 00 00

- No.: 1360
- Timestamp: 17:17:07:275_1
- RFN: 2597
- Chip: 33024
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_Security:lt_StartSecurity_UE LINE 8
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1362
- Timestamp: 17:17:07:276_0
- RFN: 2597
- Chip: 36096
- Event: Send
- PCO: CRLC
- Message: CRLC_Integrity_Activate_REQ
- Source: ts_CRLC_UL_Integrity LINE 1
- Message Structure:
CRLC_Integrity_Activate_REQ
. (IntegerType)cellId[-1] = -1
. (CN_DomainIdentity)cn_DomainIdentity[0] = 1
. IntegrityActivationInfo
. . IntegrityProtActivationInfoList
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity[-1] = 0
. . . . (IntegerType)rrc_MessageSequenceNumber[-1] = 0
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity[-1] = 1
. . . . (IntegerType)rrc_MessageSequenceNumber[-1] = 0
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity[-1] = 3
. . . . (IntegerType)rrc_MessageSequenceNumber[-1] = 0
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity[-1] = 4
. . . . (IntegerType)rrc_MessageSequenceNumber[-1] = 0
- Constraint:
ca_CRLC_UL_IntegrityActivateReq
- BinaryMessage:
30 28 02 01 ff 0a 01 01 30 20 30 06 02 01 00 02 01 00 30 06 02 01 01 02 01 00 30 06 02 01 03 02 01 00 30 06 02 01 04 02 01 00

- No.: 1363
- Timestamp: 17:17:07:276_1
- RFN: 2597
- Chip: 38144
- Event: Receive
- PCO: CRLC
- Message: CRLC_Integrity_Activate_CNF
- Source: ts_CRLC_UL_Integrity LINE 2
- Message Structure:
CRLC_Integrity_Activate_CNF
. (IntegerType)cellId[0] = -1
- Constraint:
ca_CRLC_IntegrityActivateCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1373
- Timestamp: 17:17:07:278_0
- RFN: 2598
- Chip: 7424
- Event: Send
- PCO: Dc
- Message: RRC_DataReq
- Source: ts_GMM_IdleUpdated:lt_AttachAccept LINE 4
- Message Structure:
RRC_DataReq
. (IntegerType)cellId[-1] = -1
. (SS_RB_Identity)rB_Id[-1] = 3
. (LogicChGERAN)ch[-1] = -
. (SapId)sapId[1] = -
. (SS_CN_DomainIdentity)cN_Domain[-1] = 1
. ATTACHACCEPT
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)gMMProtocolDiscriminator[4] = '1000'B
. . (MsgType)msgType[8] = '00000010'B
. . ForceToStandby
. . . (B1)spare[1] = '0'B
. . . (B3)value[3] = '000'B
. . AttachResult
. . . (B1)spare[1] = '0'B
. . . (B3)result[3] = '011'B
. . GPRS_Timer_v
. . . (B3)unit[3] = '111'B
. . . (B5)value[5] = '00000'B
. . (B4)spare[4] = '0000'B
. . RadioPriority_v
. . . (B1)spare[1] = '0'B
. . . (B3)value[3] = '100'B
. . RAI_v
. . . (OctetStringType)plmn[3] = '00F110'O
. . . (OctetStringType)lac[2] = '0001'O
. . . (OctetStringType)rac[1] = '05'O
. . PTMSI_Signature
. . . (IEI8)iei[8] = '00011001'B
. . . (OctetStringType)value[3] = 'AB1234'O
. . GPRS_Timer
. . GMM_MS_IdentityPTMSI
. . . (IEI8)iei[8] = '00011000'B
. . . (Length)iel[1] = '05'O
. . . (B4)iDigit1[4] = '1111'B
. . . (B1)oddEvenInd[1] = '0'B
. . . (B3)typeOfId[3] = '100'B
. . . (OctetStringType)otherDigits[-1] = '12345678'O
. . GMM_MS_Identity
. . . (IEI8)iei[8] = '00100011'B
. . . (Length)iel[1] = '05'O
. . . (B4)iDigit1[4] = '1111'B
. . . (B1)oddEvenInd[1] = '0'B
. . . (B3)typeOfId[3] = '100'B
. . . (OctetStringType)otherDigits[-1] = '12345678'O
. . GMM_Cause
. . GPRS_Timer
. . CellNotification
. . PLMN_List
- Constraint:
ca_PS_DataReq
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 08 02 03 e0 04 00 f1 10 00 01 05 19 ab 12 34 18 05 f4 12 34 56 78 23 05 f4 12 34 56 78

- No.: 1380
- Timestamp: 17:17:07:423_0
- RFN: 2612
- Chip: 28928
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_GMM_IdleUpdated:lt_AttachAccept LINE 5
- Message Structure:
RRC_DataInd
. (IntegerType)cellId[0] = -1
. (SS_RB_Identity)rB_Id[0] = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain[0] = 1
. (START_Value)start[0] = -
. ATTACHCOMPLETE
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)gMMProtocolDiscriminator[4] = '1000'B
. . (MsgType)msgType[8] = '00000011'B
- Constraint:
car_PS_UplinkDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 08 03

- No.: 1391
- Timestamp: 17:17:07:425_2
- RFN: 2612
- Chip: 34560
- Event: Start Timer
- Source: ts_RRC_Delay LINE 1
- Message Structure:
no details available
- Constraint:
t_Dly (1000 Ms)
- BinaryMessage:

- No.: 1395
- Timestamp: 17:17:08:415_0
- RFN: 2711
- Chip: 35328
- Event: Timeout
- Source: ts_RRC_Delay LINE 2
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 1400
- Timestamp: 17:17:08:416_0
- RFN: 2712
- Chip: 2304
- Event: Send
- PCO: UM
- Message: RLC_UM_DATA_REQ
- Source: ts_RRC_ConnRel:lt_Send_RRC_ConnectionRelease LINE 3
- Message Structure:
RLC_UM_DATA_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 1
. uM_message
. . DL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00000000000000000000000000000000"
. . . . (IntegerType)rrc_MessageSequenceNumber[-1] = 0
. . . DL_DCCH_MessageType
. . . . RRCConnectionRelease
. . . . . r3
. . . . . . RRCConnectionRelease_r3_IEs
. . . . . . . (IntegerType)rrc_TransactionIdentifier[-1] = 0
. . . . . . . (IntegerType)n_308[-1] = 1
. . . . . . . (ReleaseCause)releaseCause[0] = 0
. . . . . . . Rplmn_Information
. . . . . . laterNonCriticalExtensions
. (BooleanType)specialLI = FALSE
- Constraint:
cas_RRC_ConnRelDCCH
- BinaryMessage:
30 10 02 01 ff 02 01 01 80 00 00 00 03 c8 00 01 01 00

- No.: 1404
- Timestamp: 17:17:08:544_0
- RFN: 2724
- Chip: 28928
- Event: Receive
- PCO: UM
- Message: RLC_UM_DATA_IND
- Source: ts_RRC_ConnRel:lt_Send_RRC_ConnectionRelease LINE 4
- Message Structure:
RLC_UM_DATA_IND
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 1
. IntegrityResult
. uM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "10101101101011101001000000111001"
. . . . (IntegerType)rrc_MessageSequenceNumber[4] = 1
. . . UL_DCCH_MessageType
. . . . RRCConnectionReleaseComplete
. . . . . (IntegerType)rrc_TransactionIdentifier[2] = 0
. . . . . FailureCauseWithProtErr
. . . . . laterNonCriticalExtensions
- Constraint:
car_RRC_ConnRelCmplUM
- BinaryMessage:
30 0e 02 01 ff 02 01 01 05 00 d6 d7 48 1c 8c 40

- No.: 1405
- Timestamp: 17:17:08:544_1
- RFN: 2724
- Chip: 30208
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ConnRel:lt_Send_RRC_ConnectionRelease LINE 4
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1408
- Timestamp: 17:17:08:545_0
- RFN: 2724
- Chip: 32256
- Event: Start Timer
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 1
- Message Structure:
no details available
- Constraint:
t_Dly (5000 Ms)
- BinaryMessage:

- No.: 1412
- Timestamp: 17:17:08:703_0
- RFN: 2740
- Chip: 28928
- Event: Receive
- PCO: UM
- Message: RLC_UM_DATA_IND
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 4
- Message Structure:
RLC_UM_DATA_IND
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 1
. IntegrityResult
. uM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00011100010101000111110101101001"
. . . . (IntegerType)rrc_MessageSequenceNumber[4] = 2
. . . UL_DCCH_MessageType
. . . . RRCConnectionReleaseComplete
. . . . . (IntegerType)rrc_TransactionIdentifier[2] = 0
. . . . . FailureCauseWithProtErr
. . . . . laterNonCriticalExtensions
- Constraint:
car_RRC_ConnRelCmplUM
- BinaryMessage:
30 0e 02 01 ff 02 01 01 05 00 8e 2a 3e b4 94 40

- No.: 1413
- Timestamp: 17:17:08:704_0
- RFN: 2740
- Chip: 30720
- Event: Cancel Timer
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 4
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 1414
- Timestamp: 17:17:08:704_1
- RFN: 2740
- Chip: 30976
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 4
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1420
- Timestamp: 17:17:08:705_0
- RFN: 2740
- Chip: 35328
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 1
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 01 0a 01 00 05 00

- No.: 1424
- Timestamp: 17:17:08:711_0
- RFN: 2741
- Chip: 22272
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 1427
- Timestamp: 17:17:08:712_2
- RFN: 2741
- Chip: 25600
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 2
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 02 0a 01 00 05 00

- No.: 1431
- Timestamp: 17:17:08:716_0
- RFN: 2742
- Chip: 3072
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 1434
- Timestamp: 17:17:08:717_2
- RFN: 2742
- Chip: 6912
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 3
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 03 0a 01 00 05 00

- No.: 1438
- Timestamp: 17:17:08:722_0
- RFN: 2742
- Chip: 24832
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 3
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 1441
- Timestamp: 17:17:08:723_0
- RFN: 2742
- Chip: 28160
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 4
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 04 0a 01 00 05 00

- No.: 1445
- Timestamp: 17:17:08:730_0
- RFN: 2743
- Chip: 16128
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 4
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 1448
- Timestamp: 17:17:08:731_0
- RFN: 2743
- Chip: 22016
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 1
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 136
. . . . . UL_RLC_Mode
. . . . . . UL_UM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (NoExplicitDiscard)timerBasedNoExplicit[0] = 9
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 1
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 1
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_UM_Info
- BinaryMessage:
30 22 02 01 ff 02 01 01 0a 01 00 30 17 30 0d 05 00 30 09 02 02 00 88 30 03 0a 01 09 30 06 02 01 01 02 01 01

- No.: 1452
- Timestamp: 17:17:08:736_0
- RFN: 2744
- Chip: 768
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 1453
- Timestamp: 17:17:08:737_0
- RFN: 2744
- Chip: 6912
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 3
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 2
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 2
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 2
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 02 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 13 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 02 02 01 02

- No.: 1457
- Timestamp: 17:17:08:745_0
- RFN: 2744
- Chip: 38144
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 4
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 1458
- Timestamp: 17:17:08:747_0
- RFN: 2745
- Chip: 5888
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 5
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 3
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 3
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 3
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 03 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 13 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 03 02 01 03

- No.: 1462
- Timestamp: 17:17:08:756_0
- RFN: 2746
- Chip: 256
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 6
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 3
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 1463
- Timestamp: 17:17:08:757_0
- RFN: 2746
- Chip: 6912
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 7
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 4
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 4
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 4
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 04 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 13 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 04 02 01 04

- No.: 1467
- Timestamp: 17:17:08:765_0
- RFN: 2747
- Chip: 512
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 8
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 4
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 1496
- Timestamp: 17:17:08:769_4
- RFN: 2747
- Chip: 14080
- Event: Start Timer
- Source: ts_RRC_Delay LINE 1
- Message Structure:
no details available
- Constraint:
t_Dly (5000 Ms)
- BinaryMessage:

- No.: 1501
- Timestamp: 17:17:08:843_0
- RFN: 2754
- Chip: 25600
- Event: Receive
- PCO: CPHY
- Message: CPHY_Out_of_Sync_IND
- Source: RRC_Def1 LINE 19
- Message Structure:
CPHY_Out_of_Sync_IND
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 20
- Constraint:
ca_OutOfSyncInd
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 1502
- Timestamp: 17:17:08:843_1
- RFN: 2754
- Chip: 26368
- Event: Cancel Timer
- Source: RRC_Def1 LINE 19
- Message Structure:
no details available
- Constraint:
t_T312
- BinaryMessage:

- No.: 1503
- Timestamp: 17:17:08:843_2
- RFN: 2754
- Chip: 27136
- Event: Default
- Source: RRC_Def1 LINE 0
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1504
- Timestamp: 17:17:08:843_3
- RFN: 2754
- Chip: 27392
- Event: Default
- Source: ts_RRC_Delay LINE 2
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1509
- Timestamp: 17:17:13:772_0
- RFN: 3247
- Chip: 25856
- Event: Timeout
- Source: ts_RRC_Delay LINE 2
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 1522
- Timestamp: 17:17:13:774_0
- RFN: 3247
- Chip: 33792
- Event: Send
- PCO: Ut
- Message: MMI_CmdReq
- Source: ts_MMI_UE_SwitchOff LINE 2
- Message Structure:
MMI_CmdReq
. (IA5StringType)cmd[-1] = "Please switch off the UE"
- Constraint:
ca_MMI_CmdReq
- BinaryMessage:
50 6c 65 61 73 65 20 73 77 69 74 63 68 20 6f 66 66 20 20 74 68 65 20 55 45

- No.: 1526
- Timestamp: 17:17:17:925_0
- RFN: 3662
- Chip: 37120
- Event: Receive
- PCO: Ut
- Message: MMI_CmdCnf
- Source: ts_MMI_UE_SwitchOff LINE 3
- Message Structure:
MMI_CmdCnf
. (BooleanType)result = TRUE
. (IA5StringType)resultString[6] = " OK "
- Constraint:
ca_MMI_CmdCnf
- BinaryMessage:
80 0d 0a 4f 4b 0d 0a

- No.: 1546
- Timestamp: 17:17:19:122_0
- RFN: 3782
- Chip: 28160
- Event: Receive
- PCO: TM
- Message: RLC_TR_DATA_IND
- Source: ts_RRC_ConnEst:lt_RcvConnReq LINE 4
- Message Structure:
RLC_TR_DATA_IND
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 0
. tM_message
. . UL_CCCH_Message
. . . IntegrityCheckInfo
. . . UL_CCCH_MessageType
. . . . RRCConnectionRequest
. . . . . InitialUE_Identity
. . . . . . TMSI_and_LAI_GSM_MAP
. . . . . . . (BitStringType)tmsi[32] = "00010010001101000101011001111000"
. . . . . . . LAI
. . . . . . . . PLMN_Identity
. . . . . . . . . MCC
. . . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . . (IntegerType)_elem[4] = 1
. . . . . . . . . MNC
. . . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . . (IntegerType)_elem[4] = 1
. . . . . . . . (BitStringType)lac[16] = '0000000000000001'B
. . . . . (EstablishmentCause)establishmentCause[5] = 13
. . . . . (ProtocolErrorIndicator)protocolErrorIndicator[1] = 0
. . . . . MeasuredResultsOnRACH
. . . . . v3d0NonCriticalExtensions
- Constraint:
car_RRC_ConnReq
- BinaryMessage:
30 11 02 01 00 02 01 00 21 12 34 56 78 00 10 08 00 0b 40

- No.: 1550
- Timestamp: 17:17:19:131_0
- RFN: 3783
- Chip: 24064
- Event: Send
- PCO: UM
- Message: RLC_UM_DATA_REQ
- Source: ts_RRC_ConnEst:lt_Send_ConnSetUp LINE 22
- Message Structure:
RLC_UM_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 0
. uM_message
. . DL_CCCH_Message
. . . IntegrityCheckInfo
. . . DL_CCCH_MessageType
. . . . RRCConnectionSetup
. . . . . r3
. . . . . . RRCConnectionSetup_r3_IEs
. . . . . . . InitialUE_Identity
. . . . . . . . TMSI_and_LAI_GSM_MAP
. . . . . . . . . (BitStringType)tmsi[32] = "00010010001101000101011001111000"
. . . . . . . . . LAI
. . . . . . . . . . PLMN_Identity
. . . . . . . . . . . MCC
. . . . . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . . . . (IntegerType)_elem[4] = 1
. . . . . . . . . . . MNC
. . . . . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . . . . (IntegerType)_elem[4] = 1
. . . . . . . . . . (BitStringType)lac[16] = '0000000000000001'B
. . . . . . . (IntegerType)rrc_TransactionIdentifier[-1] = 0
. . . . . . . (IntegerType)activationTime[-1] = -
. . . . . . . U_RNTI
. . . . . . . . (BitStringType)srnc_Identity[12] = "000000000001"
. . . . . . . . (BitStringType)s_RNTI[20] = "00000000000000000001"
. . . . . . . (BitStringType)new_c_RNTI[16] = -
. . . . . . . (RRC_StateIndicator)rrc_StateIndicator[0] = 0
. . . . . . . (IntegerType)utran_DRX_CycleLengthCoeff[-1] = 9
. . . . . . . CapabilityUpdateRequirement
. . . . . . . . (BooleanType)ue_RadioCapabilityFDDUpdateRequirement = TRUE
. . . . . . . . (BooleanType)ue_RadioCapabilityTDDUpdateRequirement = FALSE
. . . . . . . . SystemSpecificCapUpdateReqList
. . . . . . . . . (SystemSpecificCapUpdateReq)_elem[0] = 0
. . . . . . . SRB_InformationSetupList2
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity[-1] = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_UM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 1
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex[-1] = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 1
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity[-1] = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 2
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 2
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 2
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 2
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex[-1] = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 2
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 2
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity[-1] = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 3
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 3
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 3
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 3
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex[-1] = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 3
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 3
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity[-1] = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 4
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 4
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 4
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 4
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex[-1] = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 4
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 4
. . . . . . . UL_CommonTransChInfo
. . . . . . . . TFC_Subset
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . TFCS
. . . . . . . . . . . ExplicitTFCS_Configuration
. . . . . . . . . . . . TFCS_ReconfAdd
. . . . . . . . . . . . . ctfcSize
. . . . . . . . . . . . . . ctfc2Bit
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . . . . . . . (IntegerType)ctfc2[-1] = 0
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . . . . . . . (IntegerType)ctfc2[-1] = 1
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC[-1] = 11
. . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaD[-1] = 15
. . . . . . . . . . . . . . . . . . . (IntegerType)referenceTFC_ID[-1] = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . UL_AddReconfTransChInfoList
. . . . . . . . UL_AddReconfTransChInformation
. . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType[0] = 0
. . . . . . . . . (IntegerType)transportChannelIdentity[-1] = 5
. . . . . . . . . TransportFormatSet
. . . . . . . . . . DedicatedTransChTFS
. . . . . . . . . . . tti
. . . . . . . . . . . . DedicatedDynamicTF_InfoList
. . . . . . . . . . . . . DedicatedDynamicTF_Info
. . . . . . . . . . . . . . rlc_Size
. . . . . . . . . . . . . . . BitModeRLC_SizeInfo
. . . . . . . . . . . . . . . . sizeType2
. . . . . . . . . . . . . . . . . (IntegerType)part1[-1] = 2
. . . . . . . . . . . . . . . . . (IntegerType)part2[-1] = -
. . . . . . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . LogicalChannelList
. . . . . . . . . . . SemistaticTF_Information
. . . . . . . . . . . . ChannelCodingType
. . . . . . . . . . . . . (CodingRate)convolutional[0] = 1
. . . . . . . . . . . . (IntegerType)rateMatchingAttribute[-1] = 192
. . . . . . . . . . . . (CRC_Size)crc_Size[0] = 3
. . . . . . . DL_CommonTransChInfo
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . dl_Parameters
. . . . . . . DL_AddReconfTransChInfoList
. . . . . . . . DL_AddReconfTransChInformation
. . . . . . . . . (DL_TrCH_Type)dl_TransportChannelType[0] = 0
. . . . . . . . . (IntegerType)dl_transportChannelIdentity[-1] = 10
. . . . . . . . . tfs_SignallingMode
. . . . . . . . . . UL_TransportChannelIdentity
. . . . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType[0] = 0
. . . . . . . . . . . (IntegerType)ul_TransportChannelIdentity[-1] = 5
. . . . . . . . . QualityTarget
. . . . . . . . . . (IntegerType)bler_QualityValue[-1] = -20
. . . . . . . . . TM_SignallingInfo
. . . . . . . FrequencyInfo
. . . . . . . (IntegerType)maxAllowedUL_TX_Power[-1] = -
. . . . . . . UL_ChannelRequirement
. . . . . . . . UL_DPCH_Info
. . . . . . . . . UL_DPCH_PowerControlInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (IntegerType)dpcch_PowerOffset[-1] = -40
. . . . . . . . . . . (IntegerType)pc_Preamble[-1] = 1
. . . . . . . . . . . (IntegerType)sRB_delay[-1] = 7
. . . . . . . . . . . PowerControlAlgorithm
. . . . . . . . . . . . (IntegerType)algorithm1[-1] = 1
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (ScramblingCodeType)scramblingCodeType[0] = 1
. . . . . . . . . . . (IntegerType)scramblingCode[-1] = 0
. . . . . . . . . . . (IntegerType)numberOfDPDCH[-1] = -
. . . . . . . . . . . (SpreadingFactor)spreadingFactor[0] = 4
. . . . . . . . . . . (BooleanType)tfci_Existence = TRUE
. . . . . . . . . . . (IntegerType)numberOfFBI_Bits[-1] = -
. . . . . . . . . . . (PuncturingLimit)puncturingLimit[0] = 15
. . . . . . . DL_CommonInformation
. . . . . . . . DL_DPCH_InfoCommon
. . . . . . . . . cfnHandling
. . . . . . . . . . initialise
. . . . . . . . . . . (IntegerType)cfntargetsfnframeoffset[-1] = -
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . DL_DPCH_PowerControlInfo
. . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . (DPC_Mode)dpc_Mode[0] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPilot_pdpdch[-1] = 0
. . . . . . . . . . . Dl_rate_matching_restriction
. . . . . . . . . . . SF512_AndPilot
. . . . . . . . . . . . (PilotBits128)sfd128[0] = 0
. . . . . . . . . . . (PositionFixedOrFlexible)positionFixedOrFlexible[0] = 0
. . . . . . . . . . . (BooleanType)tfci_Existence = FALSE
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . (IntegerType)defaultDPCH_OffsetValue[-1] = 459
. . . . . . . . . . DPCH_CompressedModeInfo
. . . . . . . . . . (TX_DiversityMode)tx_DiversityMode[0] = 0
. . . . . . . . . . SSDT_Information
. . . . . . . DL_InformationPerRL_List
. . . . . . . . DL_InformationPerRL
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . PrimaryCPICH_Info
. . . . . . . . . . . . (IntegerType)primaryScramblingCode[-1] = 100
. . . . . . . . . . . PDSCH_SHO_DCH_Info
. . . . . . . . . . . PDSCH_CodeMapping
. . . . . . . . . DL_DPCH_InfoPerRL
. . . . . . . . . . fdd
. . . . . . . . . . . (PCPICH_UsageForChannelEst)pCPICH_UsageForChannelEst[0] = 0
. . . . . . . . . . . (IntegerType)dpch_FrameOffset[-1] = 18
. . . . . . . . . . . SecondaryCPICH_Info
. . . . . . . . . . . DL_ChannelisationCodeList
. . . . . . . . . . . . DL_ChannelisationCode
. . . . . . . . . . . . . (IntegerType)secondaryScramblingCode[-1] = 1
. . . . . . . . . . . . . SF512_AndCodeNumber
. . . . . . . . . . . . . . (IntegerType)sf128[-1] = 0
. . . . . . . . . . . . . (ScramblingCodeChange)scramblingCodeChange[0] = 1
. . . . . . . . . . . (IntegerType)tpc_CombinationIndex[-1] = 0
. . . . . . . . . . . (SSDT_CellIdentity)ssdt_CellIdentity[0] = -
. . . . . . . . . . . (ClosedLoopTimingAdjMode)closedLoopTimingAdjMode[0] = -
. . . . . . . . . SCCPCH_InfoForFACH
. . . . . . laterNonCriticalExtensions
. (BooleanType)specialLI = TRUE
- Constraint:
cas_RRC_ConnSetup
- BinaryMessage:
30 78 02 01 00 02 01 00 30 e7 22 46 8a cf 00 02 01 00 01 00 04 00 00 4d 82 69 3a 10 10 89 0d 42 00 02 81 9e 8e 46 c9 a6 7c 9c 4e 74 20 a5 12 3a 8c 00 15 13 3d 1c 8d 93 4c f9 38 9c e8 42 52 24 b5 28 00 4a 46 7a 39 1b 26 99 f2 71 39 d0 86 b4 49 ea 70 00 d4 c8 00 06 25 2b f0 02 00 08 82 23 bf 66 08 98 95 a5 47 a2 00 00 01 3f 90 0a 14 e5 82 06 40 09 0c 28 08 01 01 ff

- No.: 1571
- Timestamp: 17:17:19:154_4
- RFN: 3785
- Chip: 33280
- Event: Start Timer
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 3
- Message Structure:
no details available
- Constraint:
t_WaitMS (13500 Ms)
- BinaryMessage:

- No.: 1578
- Timestamp: 17:17:19:372_1
- RFN: 3807
- Chip: 29184
- Event: Receive
- PCO: CPHY
- Message: CPHY_Sync_IND
- Source: RRC_DefConnEst LINE 5
- Message Structure:
CPHY_Sync_IND
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 20
- Constraint:
ca_SyncInd
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 1579
- Timestamp: 17:17:19:372_2
- RFN: 3807
- Chip: 29952
- Event: Cancel Timer
- Source: RRC_DefConnEst LINE 5
- Message Structure:
no details available
- Constraint:
t_T312
- BinaryMessage:

- No.: 1580
- Timestamp: 17:17:19:373_0
- RFN: 3807
- Chip: 30720
- Event: Default
- Source: RRC_DefConnEst LINE 0
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1581
- Timestamp: 17:17:19:373_1
- RFN: 3807
- Chip: 31232
- Event: Default
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1589
- Timestamp: 17:17:19:411_1
- RFN: 3811
- Chip: 26368
- Event: Receive
- PCO: CPHY
- Message: CPHY_Out_of_Sync_IND
- Source: RRC_DefConnEst LINE 7
- Message Structure:
CPHY_Out_of_Sync_IND
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 20
- Constraint:
ca_OutOfSyncInd
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 1590
- Timestamp: 17:17:19:412_0
- RFN: 3811
- Chip: 27392
- Event: Cancel Timer
- Source: RRC_DefConnEst LINE 7
- Message Structure:
no details available
- Constraint:
t_T312
- BinaryMessage:

- No.: 1591
- Timestamp: 17:17:19:412_1
- RFN: 3811
- Chip: 27904
- Event: Default
- Source: RRC_DefConnEst LINE 0
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1592
- Timestamp: 17:17:19:412_2
- RFN: 3811
- Chip: 28416
- Event: Default
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1600
- Timestamp: 17:17:19:422_1
- RFN: 3812
- Chip: 28416
- Event: Receive
- PCO: CPHY
- Message: CPHY_Sync_IND
- Source: RRC_DefConnEst LINE 5
- Message Structure:
CPHY_Sync_IND
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 20
- Constraint:
ca_SyncInd
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 1601
- Timestamp: 17:17:19:422_2
- RFN: 3812
- Chip: 29184
- Event: Cancel Timer
- Source: RRC_DefConnEst LINE 5
- Message Structure:
no details available
- Constraint:
t_T312
- BinaryMessage:

- No.: 1602
- Timestamp: 17:17:19:422_3
- RFN: 3812
- Chip: 29696
- Event: Default
- Source: RRC_DefConnEst LINE 0
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1603
- Timestamp: 17:17:19:422_4
- RFN: 3812
- Chip: 30208
- Event: Default
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1610
- Timestamp: 17:17:19:475_0
- RFN: 3817
- Chip: 36096
- Event: Receive
- PCO: AM
- Message: RLC_AM_DATA_IND
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
RLC_AM_DATA_IND
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 2
. IntegrityResult
. . (IntegrityStatus)integrityUsed[0] = 4294967296
. aM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . UL_DCCH_MessageType
. . . . RRCConnectionSetupComplete
. . . . . (IntegerType)rrc_TransactionIdentifier[2] = 0
. . . . . STARTList
. . . . . . STARTSingle
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity[1] = 1
. . . . . . . (BitStringType)start_Value[20] = "00000000000000000010"
. . . . . . STARTSingle
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity[1] = 0
. . . . . . . (BitStringType)start_Value[20] = "00000000000000000010"
. . . . . UE_RadioAccessCapability
. . . . . . (AccessStratumReleaseIndicator)accessStratumReleaseIndicator[0] = 0
. . . . . . PDCP_Capability
. . . . . . . (BooleanType)losslessSRNS_RelocationSupport = FALSE
. . . . . . . supportForRfc2507
. . . . . . . . (MaxHcContextSpace)supported[3] = 4
. . . . . . RLC_Capability
. . . . . . . (TotalRLC_AM_BufferSize)totalRLC_AM_BufferSize[3] = 2
. . . . . . . (MaximumRLC_WindowSize)maximumRLC_WindowSize[1] = 0
. . . . . . . (MaximumAM_EntityNumberRLC_Cap)maximumAM_EntityNumber[3] = 3
. . . . . . TransportChannelCapability
. . . . . . . DL_TransChCapability
. . . . . . . . (MaxNoBits)maxNoBitsReceived[4] = 7
. . . . . . . . (MaxNoBits)maxConvCodeBitsReceived[4] = 1
. . . . . . . . TurboSupport
. . . . . . . . . (MaxNoBits)supported[4] = 7
. . . . . . . . (MaxSimultaneousTransChsDL)maxSimultaneousTransChs[2] = 1
. . . . . . . . (IntegerType)maxSimultaneousCCTrCH_Count[3] = 1
. . . . . . . . (MaxTransportBlocksDL)maxReceivedTransportBlocks[4] = 3
. . . . . . . . (MaxNumberOfTFC_DL)maxNumberOfTFC[4] = 5
. . . . . . . . (MaxNumberOfTF)maxNumberOfTF[3] = 1
. . . . . . . UL_TransChCapability
. . . . . . . . (MaxNoBits)maxNoBitsTransmitted[4] = 3
. . . . . . . . (MaxNoBits)maxConvCodeBitsTransmitted[4] = 1
. . . . . . . . TurboSupport
. . . . . . . . . (MaxNoBits)supported[4] = 3
. . . . . . . . (MaxSimultaneousTransChsUL)maxSimultaneousTransChs[3] = 2
. . . . . . . . modeSpecificInfo
. . . . . . . . (MaxTransportBlocksUL)maxTransmittedBlocks[4] = 4
. . . . . . . . (MaxNumberOfTFC_UL)maxNumberOfTFC[4] = 5
. . . . . . . . (MaxNumberOfTF)maxNumberOfTF[3] = 0
. . . . . . RF_Capability
. . . . . . . fddRF_Capability
. . . . . . . . (IntegerType)ue_PowerClass[2] = 4
. . . . . . . . (TxRxFrequencySeparation)txRxFrequencySeparation[2] = 0
. . . . . . . tddRF_Capability
. . . . . . PhysicalChannelCapability
. . . . . . . fddPhysChCapability
. . . . . . . . DL_PhysChCapabilityFDD
. . . . . . . . . (IntegerType)maxNoDPCH_PDSCH_Codes[3] = 1
. . . . . . . . . (MaxNoPhysChBitsReceived)maxNoPhysChBitsReceived[4] = 6
. . . . . . . . . (BooleanType)supportForSF_512 = FALSE
. . . . . . . . . (BooleanType)supportOfPDSCH = FALSE
. . . . . . . . . SimultaneousSCCPCH_DPCH_Reception
. . . . . . . . UL_PhysChCapabilityFDD
. . . . . . . . . (MaxNoDPDCH_BitsTransmitted)maxNoDPDCH_BitsTransmitted[4] = 3
. . . . . . . . . (BooleanType)supportOfPCPCH = FALSE
. . . . . . . tddPhysChCapability
. . . . . . UE_MultiModeRAT_Capability
. . . . . . . MultiRAT_Capability
. . . . . . . . (BooleanType)supportOfGSM = FALSE
. . . . . . . . (BooleanType)supportOfMulticarrier = FALSE
. . . . . . . (MultiModeCapability)multiModeCapability[2] = 1
. . . . . . SecurityCapability
. . . . . . . (BitStringType)cipheringAlgorithmCap[16] = '0000000000000011'B
. . . . . . . (BitStringType)integrityProtectionAlgorithmCap[16] = '0000000000000010'B
. . . . . . UE_Positioning_Capability
. . . . . . . (BooleanType)standaloneLocMethodsSupported = FALSE
. . . . . . . (BooleanType)ue_BasedOTDOA_Supported = FALSE
. . . . . . . (NetworkAssistedGPS_Supported)networkAssistedGPS_Supported[2] = 3
. . . . . . . (BooleanType)supportForUE_GPS_TimingOfCellFrames = FALSE
. . . . . . . (BooleanType)supportForIPDL = FALSE
. . . . . . MeasurementCapability
. . . . . . . CompressedModeMeasCapability
. . . . . . . . (BooleanType)fdd_Measurements = TRUE
. . . . . . . . (BooleanType)tdd_Measurements = -
. . . . . . . . GSM_Measurements
. . . . . . . . . (BooleanType)gsm900 = TRUE
. . . . . . . . . (BooleanType)dcs1800 = TRUE
. . . . . . . . . (BooleanType)gsm1900 = TRUE
. . . . . . . . (BooleanType)multiCarrierMeasurements = FALSE
. . . . . . . CompressedModeMeasCapability
. . . . . . . . (BooleanType)fdd_Measurements = TRUE
. . . . . . . . (BooleanType)tdd_Measurements = -
. . . . . . . . GSM_Measurements
. . . . . . . . . (BooleanType)gsm900 = TRUE
. . . . . . . . . (BooleanType)dcs1800 = TRUE
. . . . . . . . . (BooleanType)gsm1900 = TRUE
. . . . . . . . (BooleanType)multiCarrierMeasurements = FALSE
. . . . . v370NonCriticalExtensions
- Constraint:
car_RRC_ConnSetupCmpl
- BinaryMessage:
30 27 02 01 ff 02 01 02 0a 05 01 00 00 00 00 4a 0c 00 00 80 00 05 62 37 1b a0 d4 98 cd 11 45 90 60 61 00 03 00 02 31 f9 f8

- No.: 1611
- Timestamp: 17:17:19:476_0
- RFN: 3818
- Chip: 4352
- Event: Cancel Timer
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
t_WaitMS
- BinaryMessage:

- No.: 1612
- Timestamp: 17:17:19:477_0
- RFN: 3818
- Chip: 4864
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1634
- Timestamp: 17:17:19:494_0
- RFN: 3819
- Chip: 32000
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_GMM_DetachOnSwitchOff:lt_Detach_NMO_I LINE 1
- Message Structure:
RRC_DataInd
. (IntegerType)cellId[0] = -1
. (SS_RB_Identity)rB_Id[0] = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain[0] = 1
. (START_Value)start[20] = '00000000000000000010'B
. DETACHREQUESTMO
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)gMMProtocolDiscriminator[4] = '1000'B
. . (MsgType)msgType[8] = '00000101'B
. . (B4)spare4[4] = '0000'B
. . DetachType
. . . (B1)powOff[1] = '1'B
. . . (B3)type[3] = '011'B
. . GMM_MS_IdentityPTMSI
. . . (IEI8)iei[8] = '00011000'B
. . . (Length)iel[1] = '05'O
. . . (B4)iDigit1[4] = '1111'B
. . . (B1)oddEvenInd[1] = '0'B
. . . (B3)typeOfId[3] = '100'B
. . . (OctetStringType)otherDigits[4] = '12345678'O
. . PTMSI_Signature_tlv
. . . (IEI8)iei[8] = '00011001'B
. . . (Length)iel[1] = '03'O
. . . (OctetStringType)value[3] = 'AB1234'O
- Constraint:
car_PS_InitDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 03 04 04 00 00 20 08 05 0b 18 05 f4 12 34 56 78 19 03 ab 12 34

- No.: 1635
- Timestamp: 17:17:19:494_1
- RFN: 3819
- Chip: 33536
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_GMM_DetachOnSwitchOff:lt_Detach_NMO_I LINE 1
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1644
- Timestamp: 17:17:19:495_5
- RFN: 3819
- Chip: 37888
- Event: Start Timer
- Source: ts_RRC_Delay LINE 1
- Message Structure:
no details available
- Constraint:
t_Dly (1000 Ms)
- BinaryMessage:

- No.: 1648
- Timestamp: 17:17:20:490_0
- RFN: 3919
- Chip: 18432
- Event: Timeout
- Source: ts_RRC_Delay LINE 2
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 1653
- Timestamp: 17:17:20:491_0
- RFN: 3919
- Chip: 23296
- Event: Send
- PCO: UM
- Message: RLC_UM_DATA_REQ
- Source: ts_RRC_ConnRel_AfterSwitchOff:lt_Send_RRC_ConnectionRelease LINE 3
- Message Structure:
RLC_UM_DATA_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 1
. uM_message
. . DL_DCCH_Message
. . . IntegrityCheckInfo
. . . DL_DCCH_MessageType
. . . . RRCConnectionRelease
. . . . . r3
. . . . . . RRCConnectionRelease_r3_IEs
. . . . . . . (IntegerType)rrc_TransactionIdentifier[-1] = 0
. . . . . . . (IntegerType)n_308[-1] = 1
. . . . . . . (ReleaseCause)releaseCause[0] = 0
. . . . . . . Rplmn_Information
. . . . . . laterNonCriticalExtensions
. (BooleanType)specialLI = FALSE
- Constraint:
cas_RRC_ConnRelDCCH
- BinaryMessage:
30 0c 02 01 ff 02 01 01 3c 80 00 01 01 00

- No.: 1655
- Timestamp: 17:17:20:492_0
- RFN: 3919
- Chip: 25856
- Event: Start Timer
- Source: ts_RRC_ConnRel_AfterSwitchOff:lt_Send_RRC_ConnectionRelease LINE 4
- Message Structure:
no details available
- Constraint:
t_Dly (1000 Ms)
- BinaryMessage:

- No.: 1659
- Timestamp: 17:17:20:612_0
- RFN: 3931
- Chip: 29952
- Event: Receive
- PCO: UM
- Message: RLC_UM_DATA_IND
- Source: ts_RRC_ConnRel_AfterSwitchOff:lt_Send_RRC_ConnectionRelease LINE 6
- Message Structure:
RLC_UM_DATA_IND
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 1
. IntegrityResult
. uM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . UL_DCCH_MessageType
. . . . RRCConnectionReleaseComplete
. . . . . (IntegerType)rrc_TransactionIdentifier[2] = 0
. . . . . FailureCauseWithProtErr
. . . . . laterNonCriticalExtensions
- Constraint:
car_RRC_ConnRelCmplUM
- BinaryMessage:
30 0a 02 01 ff 02 01 01 05 00 44 00

- No.: 1660
- Timestamp: 17:17:20:613_0
- RFN: 3931
- Chip: 31232
- Event: Cancel Timer
- Source: ts_RRC_ConnRel_AfterSwitchOff:lt_Send_RRC_ConnectionRelease LINE 6
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 1661
- Timestamp: 17:17:20:613_1
- RFN: 3931
- Chip: 31488
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ConnRel_AfterSwitchOff:lt_Send_RRC_ConnectionRelease LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1664
- Timestamp: 17:17:20:613_4
- RFN: 3931
- Chip: 33536
- Event: Start Timer
- Source: ts_RRC_ConnRel_AfterSwitchOff:lt_RptRcvConnRel LINE 1
- Message Structure:
no details available
- Constraint:
t_Dly (5000 Ms)
- BinaryMessage:

- No.: 1668
- Timestamp: 17:17:20:773_0
- RFN: 3947
- Chip: 29952
- Event: Receive
- PCO: UM
- Message: RLC_UM_DATA_IND
- Source: ts_RRC_ConnRel_AfterSwitchOff:lt_RptRcvConnRel LINE 4
- Message Structure:
RLC_UM_DATA_IND
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 1
. IntegrityResult
. uM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . UL_DCCH_MessageType
. . . . RRCConnectionReleaseComplete
. . . . . (IntegerType)rrc_TransactionIdentifier[2] = 0
. . . . . FailureCauseWithProtErr
. . . . . laterNonCriticalExtensions
- Constraint:
car_RRC_ConnRelCmplUM
- BinaryMessage:
30 0a 02 01 ff 02 01 01 05 00 44 00

- No.: 1669
- Timestamp: 17:17:20:773_1
- RFN: 3947
- Chip: 31232
- Event: Cancel Timer
- Source: ts_RRC_ConnRel_AfterSwitchOff:lt_RptRcvConnRel LINE 4
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 1670
- Timestamp: 17:17:20:773_2
- RFN: 3947
- Chip: 31744
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ConnRel_AfterSwitchOff:lt_RptRcvConnRel LINE 4
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1676
- Timestamp: 17:17:20:775_0
- RFN: 3947
- Chip: 36352
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 1
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 01 0a 01 00 05 00

- No.: 1680
- Timestamp: 17:17:20:781_0
- RFN: 3948
- Chip: 22016
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 1683
- Timestamp: 17:17:20:782_0
- RFN: 3948
- Chip: 25088
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 2
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 02 0a 01 00 05 00

- No.: 1687
- Timestamp: 17:17:20:786_0
- RFN: 3949
- Chip: 2304
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 1690
- Timestamp: 17:17:20:787_0
- RFN: 3949
- Chip: 6144
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 3
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 03 0a 01 00 05 00

- No.: 1694
- Timestamp: 17:17:20:792_0
- RFN: 3949
- Chip: 25600
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 3
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 1697
- Timestamp: 17:17:20:793_0
- RFN: 3949
- Chip: 29440
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 4
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 04 0a 01 00 05 00

- No.: 1701
- Timestamp: 17:17:20:799_0
- RFN: 3950
- Chip: 16640
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 4
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 1704
- Timestamp: 17:17:20:801_0
- RFN: 3950
- Chip: 23296
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 1
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 136
. . . . . UL_RLC_Mode
. . . . . . UL_UM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (NoExplicitDiscard)timerBasedNoExplicit[0] = 9
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 1
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 1
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_UM_Info
- BinaryMessage:
30 22 02 01 ff 02 01 01 0a 01 00 30 17 30 0d 05 00 30 09 02 02 00 88 30 03 0a 01 09 30 06 02 01 01 02 01 01

- No.: 1708
- Timestamp: 17:17:20:805_0
- RFN: 3951
- Chip: 512
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 1709
- Timestamp: 17:17:20:807_0
- RFN: 3951
- Chip: 7424
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 3
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 2
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 2
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 2
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 02 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 13 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 02 02 01 02

- No.: 1713
- Timestamp: 17:17:20:815_0
- RFN: 3952
- Chip: 768
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 4
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 1714
- Timestamp: 17:17:20:817_0
- RFN: 3952
- Chip: 7936
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 5
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 3
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 3
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 3
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 03 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 13 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 03 02 01 03

- No.: 1718
- Timestamp: 17:17:20:825_0
- RFN: 3952
- Chip: 37632
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 6
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 3
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 1719
- Timestamp: 17:17:20:826_0
- RFN: 3953
- Chip: 5632
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 7
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 4
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 4
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 4
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 04 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 13 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 04 02 01 04

- No.: 1723
- Timestamp: 17:17:20:835_0
- RFN: 3954
- Chip: 1536
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 8
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 4
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 1747
- Timestamp: 17:17:20:838_6
- RFN: 3954
- Chip: 13056
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: tc_12_4_1_4c2:lt_TestBody LINE 1
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1753
- Timestamp: 17:17:20:839_4
- RFN: 3954
- Chip: 17408
- Event: Send
- PCO: Ut
- Message: MMI_CmdReq
- Source: ts_MMI_UE_SwitchOn LINE 2
- Message Structure:
MMI_CmdReq
. (IA5StringType)cmd[-1] = "Please switch on the UE"
- Constraint:
ca_MMI_CmdReq
- BinaryMessage:
50 6c 65 61 73 65 20 73 77 69 74 63 68 20 6f 6e 20 74 68 65 20 55 45

- No.: 1760
- Timestamp: 17:17:20:991_0
- RFN: 3969
- Chip: 26624
- Event: Receive
- PCO: Ut
- Message: MMI_CmdCnf
- Source: ts_MMI_UE_SwitchOn LINE 3
- Message Structure:
MMI_CmdCnf
. (BooleanType)result = TRUE
. (IA5StringType)resultString[6] = " OK "
- Constraint:
ca_MMI_CmdCnf
- BinaryMessage:
80 0d 0a 4f 4b 0d 0a

- No.: 1779
- Timestamp: 17:17:20:994_1
- RFN: 3969
- Chip: 36352
- Event: Receive
- PCO: CPHY
- Message: CPHY_Out_of_Sync_IND
- Source: RRC_DefConnEst LINE 7
- Message Structure:
CPHY_Out_of_Sync_IND
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 20
- Constraint:
ca_OutOfSyncInd
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 1780
- Timestamp: 17:17:20:994_2
- RFN: 3969
- Chip: 37120
- Event: Cancel Timer
- Source: RRC_DefConnEst LINE 7
- Message Structure:
no details available
- Constraint:
t_T312
- BinaryMessage:

- No.: 1781
- Timestamp: 17:17:20:994_3
- RFN: 3969
- Chip: 37632
- Event: Default
- Source: RRC_DefConnEst LINE 0
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1782
- Timestamp: 17:17:20:994_4
- RFN: 3969
- Chip: 38144
- Event: Default
- Source: ts_RRC_ConnEst:lt_RcvConnReq LINE 2
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1787
- Timestamp: 17:17:40:969_0
- RFN: 5967
- Chip: 23808
- Event: Receive
- PCO: TM
- Message: RLC_TR_DATA_IND
- Source: ts_RRC_ConnEst:lt_RcvConnReq LINE 2
- Message Structure:
RLC_TR_DATA_IND
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 0
. tM_message
. . UL_CCCH_Message
. . . IntegrityCheckInfo
. . . UL_CCCH_MessageType
. . . . RRCConnectionRequest
. . . . . InitialUE_Identity
. . . . . . TMSI_and_LAI_GSM_MAP
. . . . . . . (BitStringType)tmsi[32] = "00010010001101000101011001111000"
. . . . . . . LAI
. . . . . . . . PLMN_Identity
. . . . . . . . . MCC
. . . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . . (IntegerType)_elem[4] = 1
. . . . . . . . . MNC
. . . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . . (IntegerType)_elem[4] = 1
. . . . . . . . (BitStringType)lac[16] = '0000000000000001'B
. . . . . (EstablishmentCause)establishmentCause[5] = 12
. . . . . (ProtocolErrorIndicator)protocolErrorIndicator[1] = 0
. . . . . MeasuredResultsOnRACH
. . . . . v3d0NonCriticalExtensions
- Constraint:
car_RRC_ConnReq
- BinaryMessage:
30 11 02 01 00 02 01 00 21 12 34 56 78 00 10 08 00 0b 00

- No.: 1791
- Timestamp: 17:17:40:979_0
- RFN: 5968
- Chip: 25600
- Event: Send
- PCO: UM
- Message: RLC_UM_DATA_REQ
- Source: ts_RRC_ConnEst:lt_Send_ConnSetUp LINE 22
- Message Structure:
RLC_UM_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 0
. uM_message
. . DL_CCCH_Message
. . . IntegrityCheckInfo
. . . DL_CCCH_MessageType
. . . . RRCConnectionSetup
. . . . . r3
. . . . . . RRCConnectionSetup_r3_IEs
. . . . . . . InitialUE_Identity
. . . . . . . . TMSI_and_LAI_GSM_MAP
. . . . . . . . . (BitStringType)tmsi[32] = "00010010001101000101011001111000"
. . . . . . . . . LAI
. . . . . . . . . . PLMN_Identity
. . . . . . . . . . . MCC
. . . . . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . . . . (IntegerType)_elem[4] = 1
. . . . . . . . . . . MNC
. . . . . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . . . . (IntegerType)_elem[4] = 1
. . . . . . . . . . (BitStringType)lac[16] = '0000000000000001'B
. . . . . . . (IntegerType)rrc_TransactionIdentifier[-1] = 0
. . . . . . . (IntegerType)activationTime[-1] = -
. . . . . . . U_RNTI
. . . . . . . . (BitStringType)srnc_Identity[12] = "000000000001"
. . . . . . . . (BitStringType)s_RNTI[20] = "00000000000000000001"
. . . . . . . (BitStringType)new_c_RNTI[16] = -
. . . . . . . (RRC_StateIndicator)rrc_StateIndicator[0] = 0
. . . . . . . (IntegerType)utran_DRX_CycleLengthCoeff[-1] = 9
. . . . . . . CapabilityUpdateRequirement
. . . . . . . . (BooleanType)ue_RadioCapabilityFDDUpdateRequirement = TRUE
. . . . . . . . (BooleanType)ue_RadioCapabilityTDDUpdateRequirement = FALSE
. . . . . . . . SystemSpecificCapUpdateReqList
. . . . . . . . . (SystemSpecificCapUpdateReq)_elem[0] = 0
. . . . . . . SRB_InformationSetupList2
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity[-1] = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_UM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 1
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex[-1] = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 1
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity[-1] = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 2
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 2
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 2
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 2
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex[-1] = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 2
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 2
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity[-1] = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 3
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 3
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 3
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 3
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex[-1] = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 3
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 3
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity[-1] = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 4
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 4
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 4
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 4
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex[-1] = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 4
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 4
. . . . . . . UL_CommonTransChInfo
. . . . . . . . TFC_Subset
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . TFCS
. . . . . . . . . . . ExplicitTFCS_Configuration
. . . . . . . . . . . . TFCS_ReconfAdd
. . . . . . . . . . . . . ctfcSize
. . . . . . . . . . . . . . ctfc2Bit
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . . . . . . . (IntegerType)ctfc2[-1] = 0
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . . . . . . . (IntegerType)ctfc2[-1] = 1
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC[-1] = 11
. . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaD[-1] = 15
. . . . . . . . . . . . . . . . . . . (IntegerType)referenceTFC_ID[-1] = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . UL_AddReconfTransChInfoList
. . . . . . . . UL_AddReconfTransChInformation
. . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType[0] = 0
. . . . . . . . . (IntegerType)transportChannelIdentity[-1] = 5
. . . . . . . . . TransportFormatSet
. . . . . . . . . . DedicatedTransChTFS
. . . . . . . . . . . tti
. . . . . . . . . . . . DedicatedDynamicTF_InfoList
. . . . . . . . . . . . . DedicatedDynamicTF_Info
. . . . . . . . . . . . . . rlc_Size
. . . . . . . . . . . . . . . BitModeRLC_SizeInfo
. . . . . . . . . . . . . . . . sizeType2
. . . . . . . . . . . . . . . . . (IntegerType)part1[-1] = 2
. . . . . . . . . . . . . . . . . (IntegerType)part2[-1] = -
. . . . . . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . LogicalChannelList
. . . . . . . . . . . SemistaticTF_Information
. . . . . . . . . . . . ChannelCodingType
. . . . . . . . . . . . . (CodingRate)convolutional[0] = 1
. . . . . . . . . . . . (IntegerType)rateMatchingAttribute[-1] = 192
. . . . . . . . . . . . (CRC_Size)crc_Size[0] = 3
. . . . . . . DL_CommonTransChInfo
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . dl_Parameters
. . . . . . . DL_AddReconfTransChInfoList
. . . . . . . . DL_AddReconfTransChInformation
. . . . . . . . . (DL_TrCH_Type)dl_TransportChannelType[0] = 0
. . . . . . . . . (IntegerType)dl_transportChannelIdentity[-1] = 10
. . . . . . . . . tfs_SignallingMode
. . . . . . . . . . UL_TransportChannelIdentity
. . . . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType[0] = 0
. . . . . . . . . . . (IntegerType)ul_TransportChannelIdentity[-1] = 5
. . . . . . . . . QualityTarget
. . . . . . . . . . (IntegerType)bler_QualityValue[-1] = -20
. . . . . . . . . TM_SignallingInfo
. . . . . . . FrequencyInfo
. . . . . . . (IntegerType)maxAllowedUL_TX_Power[-1] = -
. . . . . . . UL_ChannelRequirement
. . . . . . . . UL_DPCH_Info
. . . . . . . . . UL_DPCH_PowerControlInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (IntegerType)dpcch_PowerOffset[-1] = -40
. . . . . . . . . . . (IntegerType)pc_Preamble[-1] = 1
. . . . . . . . . . . (IntegerType)sRB_delay[-1] = 7
. . . . . . . . . . . PowerControlAlgorithm
. . . . . . . . . . . . (IntegerType)algorithm1[-1] = 1
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (ScramblingCodeType)scramblingCodeType[0] = 1
. . . . . . . . . . . (IntegerType)scramblingCode[-1] = 0
. . . . . . . . . . . (IntegerType)numberOfDPDCH[-1] = -
. . . . . . . . . . . (SpreadingFactor)spreadingFactor[0] = 4
. . . . . . . . . . . (BooleanType)tfci_Existence = TRUE
. . . . . . . . . . . (IntegerType)numberOfFBI_Bits[-1] = -
. . . . . . . . . . . (PuncturingLimit)puncturingLimit[0] = 15
. . . . . . . DL_CommonInformation
. . . . . . . . DL_DPCH_InfoCommon
. . . . . . . . . cfnHandling
. . . . . . . . . . initialise
. . . . . . . . . . . (IntegerType)cfntargetsfnframeoffset[-1] = -
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . DL_DPCH_PowerControlInfo
. . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . (DPC_Mode)dpc_Mode[0] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPilot_pdpdch[-1] = 0
. . . . . . . . . . . Dl_rate_matching_restriction
. . . . . . . . . . . SF512_AndPilot
. . . . . . . . . . . . (PilotBits128)sfd128[0] = 0
. . . . . . . . . . . (PositionFixedOrFlexible)positionFixedOrFlexible[0] = 0
. . . . . . . . . . . (BooleanType)tfci_Existence = FALSE
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . (IntegerType)defaultDPCH_OffsetValue[-1] = 459
. . . . . . . . . . DPCH_CompressedModeInfo
. . . . . . . . . . (TX_DiversityMode)tx_DiversityMode[0] = 0
. . . . . . . . . . SSDT_Information
. . . . . . . DL_InformationPerRL_List
. . . . . . . . DL_InformationPerRL
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . PrimaryCPICH_Info
. . . . . . . . . . . . (IntegerType)primaryScramblingCode[-1] = 100
. . . . . . . . . . . PDSCH_SHO_DCH_Info
. . . . . . . . . . . PDSCH_CodeMapping
. . . . . . . . . DL_DPCH_InfoPerRL
. . . . . . . . . . fdd
. . . . . . . . . . . (PCPICH_UsageForChannelEst)pCPICH_UsageForChannelEst[0] = 0
. . . . . . . . . . . (IntegerType)dpch_FrameOffset[-1] = 18
. . . . . . . . . . . SecondaryCPICH_Info
. . . . . . . . . . . DL_ChannelisationCodeList
. . . . . . . . . . . . DL_ChannelisationCode
. . . . . . . . . . . . . (IntegerType)secondaryScramblingCode[-1] = 1
. . . . . . . . . . . . . SF512_AndCodeNumber
. . . . . . . . . . . . . . (IntegerType)sf128[-1] = 0
. . . . . . . . . . . . . (ScramblingCodeChange)scramblingCodeChange[0] = 1
. . . . . . . . . . . (IntegerType)tpc_CombinationIndex[-1] = 0
. . . . . . . . . . . (SSDT_CellIdentity)ssdt_CellIdentity[0] = -
. . . . . . . . . . . (ClosedLoopTimingAdjMode)closedLoopTimingAdjMode[0] = -
. . . . . . . . . SCCPCH_InfoForFACH
. . . . . . laterNonCriticalExtensions
. (BooleanType)specialLI = TRUE
- Constraint:
cas_RRC_ConnSetup
- BinaryMessage:
30 78 02 01 00 02 01 00 30 e7 22 46 8a cf 00 02 01 00 01 00 04 00 00 4d 82 69 3a 10 10 89 0d 42 00 02 81 9e 8e 46 c9 a6 7c 9c 4e 74 20 a5 12 3a 8c 00 15 13 3d 1c 8d 93 4c f9 38 9c e8 42 52 24 b5 28 00 4a 46 7a 39 1b 26 99 f2 71 39 d0 86 b4 49 ea 70 00 d4 c8 00 06 25 2b f0 02 00 08 82 23 bf 66 08 98 95 a5 47 a2 00 00 01 3f 90 0a 14 e5 82 06 40 09 0c 28 08 01 01 ff

- No.: 1812
- Timestamp: 17:17:41:002_0
- RFN: 5970
- Chip: 34048
- Event: Start Timer
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 3
- Message Structure:
no details available
- Constraint:
t_WaitMS (13500 Ms)
- BinaryMessage:

- No.: 1819
- Timestamp: 17:17:41:191_1
- RFN: 5989
- Chip: 29696
- Event: Receive
- PCO: CPHY
- Message: CPHY_Sync_IND
- Source: RRC_DefConnEst LINE 5
- Message Structure:
CPHY_Sync_IND
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 20
- Constraint:
ca_SyncInd
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 1820
- Timestamp: 17:17:41:191_2
- RFN: 5989
- Chip: 30464
- Event: Cancel Timer
- Source: RRC_DefConnEst LINE 5
- Message Structure:
no details available
- Constraint:
t_T312
- BinaryMessage:

- No.: 1821
- Timestamp: 17:17:41:191_3
- RFN: 5989
- Chip: 31232
- Event: Default
- Source: RRC_DefConnEst LINE 0
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1822
- Timestamp: 17:17:41:191_4
- RFN: 5989
- Chip: 31488
- Event: Default
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1829
- Timestamp: 17:17:41:292_0
- RFN: 5999
- Chip: 36608
- Event: Receive
- PCO: AM
- Message: RLC_AM_DATA_IND
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
RLC_AM_DATA_IND
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 2
. IntegrityResult
. . (IntegrityStatus)integrityUsed[0] = 4294967296
. aM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . UL_DCCH_MessageType
. . . . RRCConnectionSetupComplete
. . . . . (IntegerType)rrc_TransactionIdentifier[2] = 0
. . . . . STARTList
. . . . . . STARTSingle
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity[1] = 1
. . . . . . . (BitStringType)start_Value[20] = "00000000000000000010"
. . . . . . STARTSingle
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity[1] = 0
. . . . . . . (BitStringType)start_Value[20] = "00000000000000000010"
. . . . . UE_RadioAccessCapability
. . . . . . (AccessStratumReleaseIndicator)accessStratumReleaseIndicator[0] = 0
. . . . . . PDCP_Capability
. . . . . . . (BooleanType)losslessSRNS_RelocationSupport = FALSE
. . . . . . . supportForRfc2507
. . . . . . . . (MaxHcContextSpace)supported[3] = 4
. . . . . . RLC_Capability
. . . . . . . (TotalRLC_AM_BufferSize)totalRLC_AM_BufferSize[3] = 2
. . . . . . . (MaximumRLC_WindowSize)maximumRLC_WindowSize[1] = 0
. . . . . . . (MaximumAM_EntityNumberRLC_Cap)maximumAM_EntityNumber[3] = 3
. . . . . . TransportChannelCapability
. . . . . . . DL_TransChCapability
. . . . . . . . (MaxNoBits)maxNoBitsReceived[4] = 7
. . . . . . . . (MaxNoBits)maxConvCodeBitsReceived[4] = 1
. . . . . . . . TurboSupport
. . . . . . . . . (MaxNoBits)supported[4] = 7
. . . . . . . . (MaxSimultaneousTransChsDL)maxSimultaneousTransChs[2] = 1
. . . . . . . . (IntegerType)maxSimultaneousCCTrCH_Count[3] = 1
. . . . . . . . (MaxTransportBlocksDL)maxReceivedTransportBlocks[4] = 3
. . . . . . . . (MaxNumberOfTFC_DL)maxNumberOfTFC[4] = 5
. . . . . . . . (MaxNumberOfTF)maxNumberOfTF[3] = 1
. . . . . . . UL_TransChCapability
. . . . . . . . (MaxNoBits)maxNoBitsTransmitted[4] = 3
. . . . . . . . (MaxNoBits)maxConvCodeBitsTransmitted[4] = 1
. . . . . . . . TurboSupport
. . . . . . . . . (MaxNoBits)supported[4] = 3
. . . . . . . . (MaxSimultaneousTransChsUL)maxSimultaneousTransChs[3] = 2
. . . . . . . . modeSpecificInfo
. . . . . . . . (MaxTransportBlocksUL)maxTransmittedBlocks[4] = 4
. . . . . . . . (MaxNumberOfTFC_UL)maxNumberOfTFC[4] = 5
. . . . . . . . (MaxNumberOfTF)maxNumberOfTF[3] = 0
. . . . . . RF_Capability
. . . . . . . fddRF_Capability
. . . . . . . . (IntegerType)ue_PowerClass[2] = 4
. . . . . . . . (TxRxFrequencySeparation)txRxFrequencySeparation[2] = 0
. . . . . . . tddRF_Capability
. . . . . . PhysicalChannelCapability
. . . . . . . fddPhysChCapability
. . . . . . . . DL_PhysChCapabilityFDD
. . . . . . . . . (IntegerType)maxNoDPCH_PDSCH_Codes[3] = 1
. . . . . . . . . (MaxNoPhysChBitsReceived)maxNoPhysChBitsReceived[4] = 6
. . . . . . . . . (BooleanType)supportForSF_512 = FALSE
. . . . . . . . . (BooleanType)supportOfPDSCH = FALSE
. . . . . . . . . SimultaneousSCCPCH_DPCH_Reception
. . . . . . . . UL_PhysChCapabilityFDD
. . . . . . . . . (MaxNoDPDCH_BitsTransmitted)maxNoDPDCH_BitsTransmitted[4] = 3
. . . . . . . . . (BooleanType)supportOfPCPCH = FALSE
. . . . . . . tddPhysChCapability
. . . . . . UE_MultiModeRAT_Capability
. . . . . . . MultiRAT_Capability
. . . . . . . . (BooleanType)supportOfGSM = FALSE
. . . . . . . . (BooleanType)supportOfMulticarrier = FALSE
. . . . . . . (MultiModeCapability)multiModeCapability[2] = 1
. . . . . . SecurityCapability
. . . . . . . (BitStringType)cipheringAlgorithmCap[16] = '0000000000000011'B
. . . . . . . (BitStringType)integrityProtectionAlgorithmCap[16] = '0000000000000010'B
. . . . . . UE_Positioning_Capability
. . . . . . . (BooleanType)standaloneLocMethodsSupported = FALSE
. . . . . . . (BooleanType)ue_BasedOTDOA_Supported = FALSE
. . . . . . . (NetworkAssistedGPS_Supported)networkAssistedGPS_Supported[2] = 3
. . . . . . . (BooleanType)supportForUE_GPS_TimingOfCellFrames = FALSE
. . . . . . . (BooleanType)supportForIPDL = FALSE
. . . . . . MeasurementCapability
. . . . . . . CompressedModeMeasCapability
. . . . . . . . (BooleanType)fdd_Measurements = TRUE
. . . . . . . . (BooleanType)tdd_Measurements = -
. . . . . . . . GSM_Measurements
. . . . . . . . . (BooleanType)gsm900 = TRUE
. . . . . . . . . (BooleanType)dcs1800 = TRUE
. . . . . . . . . (BooleanType)gsm1900 = TRUE
. . . . . . . . (BooleanType)multiCarrierMeasurements = FALSE
. . . . . . . CompressedModeMeasCapability
. . . . . . . . (BooleanType)fdd_Measurements = TRUE
. . . . . . . . (BooleanType)tdd_Measurements = -
. . . . . . . . GSM_Measurements
. . . . . . . . . (BooleanType)gsm900 = TRUE
. . . . . . . . . (BooleanType)dcs1800 = TRUE
. . . . . . . . . (BooleanType)gsm1900 = TRUE
. . . . . . . . (BooleanType)multiCarrierMeasurements = FALSE
. . . . . v370NonCriticalExtensions
- Constraint:
car_RRC_ConnSetupCmpl
- BinaryMessage:
30 27 02 01 ff 02 01 02 0a 05 01 00 00 00 00 4a 0c 00 00 80 00 05 62 37 1b a0 d4 98 cd 11 45 90 60 61 00 03 00 02 31 f9 f8

- No.: 1830
- Timestamp: 17:17:41:294_0
- RFN: 6000
- Chip: 5120
- Event: Cancel Timer
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
t_WaitMS
- BinaryMessage:

- No.: 1831
- Timestamp: 17:17:41:294_1
- RFN: 6000
- Chip: 5376
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1850
- Timestamp: 17:17:41:311_0
- RFN: 6001
- Chip: 32512
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_GMM_TriggerPSRegistrationAtSwitchOn_NMO_I LINE 5
- Message Structure:
RRC_DataInd
. (IntegerType)cellId[0] = -1
. (SS_RB_Identity)rB_Id[0] = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain[0] = 0
. (START_Value)start[20] = '00000000000000000010'B
. LOCATIONUPDATINGREQUEST
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)mMProtocolDiscriminator[4] = '0101'B
. . (MsgType)msgType[8] = '00001000'B
. . CiphKeySeqNum
. . . (B1)spare1[1] = '0'B
. . . (KeySeq)keySeq[3] = '000'B
. . LocUpdType
. . . (B1)fOR[1] = '0'B
. . . (B1)spare1[1] = '0'B
. . . (B2)lUT[2] = '10'B
. . LocAreaId_v
. . . (OctetStringType)plmn[3] = '00F110'O
. . . (OctetStringType)lac[2] = '0001'O
. . MS_Clsmk1
. . . (B1)spare1[1] = '0'B
. . . (B2)revLvl[2] = '10'B
. . . (B1)eSIND[1] = '0'B
. . . (B1)a5_1[1] = '1'B
. . . (B3)rFPwrCap[3] = '111'B
. . MS_Identity_lv
. . . (Length)iel[1] = '05'O
. . . (B4)iDigit1[4] = '1111'B
. . . (B1)oddEvenInd[1] = '0'B
. . . (B3)typeOfId[3] = '100'B
. . . (OctetStringType)otherDigits[4] = '12345678'O
. . MS_Clsmk2
. . . (IEI8)iei[8] = '00110011'B
. . . (Length)iel[1] = '03'O
. . . (B1)spare1_1[1] = '0'B
. . . (B2)revLvl[2] = '10'B
. . . (B1)eSIND[1] = '0'B
. . . (B1)a5_1[1] = '1'B
. . . (B3)rFPwrCap[3] = '111'B
. . . (B1)spare1_2[1] = '0'B
. . . (B1)pSCap[1] = '0'B
. . . (B2)sSSI[2] = '01'B
. . . (B1)sMCap[1] = '1'B
. . . (B1)vBS[1] = '0'B
. . . (B1)vGCS[1] = '0'B
. . . (B1)fC[1] = '0'B
. . . (B1)cM3[1] = '1'B
. . . (B1)spare1_3[1] = '0'B
. . . (B1)lCSVA[1] = '1'B
. . . (B1)uCS2[1] = '0'B
. . . (B1)soLSA[1] = '0'B
. . . (B1)cMSP[1] = '0'B
. . . (B1)a5_3[1] = '0'B
. . . (B1)a5_2[1] = '0'B
- Constraint:
car_InitDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 00 03 04 04 00 00 20 05 08 02 00 f1 10 00 01 4f 05 f4 12 34 56 78 33 03 4f 18 a0

- No.: 1886
- Timestamp: 17:17:41:317_0
- RFN: 6002
- Chip: 17152
- Event: Send
- PCO: Dc
- Message: RRC_DataReq
- Source: ts_MM_Authentication LINE 2
- Message Structure:
RRC_DataReq
. (IntegerType)cellId[-1] = -1
. (SS_RB_Identity)rB_Id[-1] = 3
. (LogicChGERAN)ch[-1] = -
. (SapId)sapId[1] = -
. (SS_CN_DomainIdentity)cN_Domain[-1] = 0
. AUTHENTICATIONREQUEST
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)mMProtocolDiscriminator[4] = '0101'B
. . (MsgType)msgType[8] = '00010010'B
. . (B4)spare4[4] = '0000'B
. . CiphKeySeqNum
. . . (B1)spare1[1] = '0'B
. . . (KeySeq)keySeq[3] = '001'B
. . (MM_RAND)rAND[128] = '01010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101'B
. . AUTN
. . . (IEI8)iei[8] = '00100000'B
. . . (Length)iel[1] = '10'O
. . . (BitStringType)aUTN[128] = '01010110010100010101000001010011010100100101110100000000000000000101010101010100010101110101011001010001010100000101001101010010'B
- Constraint:
ca_DataReq
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 00 05 12 01 55 55 55 55 55 55 55 55 55 55 55 55 55 55 55 55 20 10 56 51 50 53 52 5d 00 00 55 54 57 56 51 50 53 52

- No.: 1890
- Timestamp: 17:17:41:591_0
- RFN: 6029
- Chip: 30464
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_MM_Authentication LINE 3
- Message Structure:
RRC_DataInd
. (IntegerType)cellId[0] = -1
. (SS_RB_Identity)rB_Id[0] = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain[0] = 0
. (START_Value)start[0] = -
. AUTHENTICATIONRESPONSE
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)mMProtocolDiscriminator[4] = '0101'B
. . (MsgType)msgType[8] = '01010100'B
. . (AuthRsp)authRsp[32] = '01010101010101000101011101010110'B
. . AuthRspExt
. . . (IEI8)iei[8] = '00100001'B
. . . (Length)iel[1] = '0C'O
. . . (BitStringType)rES[96] = '010100010101000001010011010100100101110101011100010111110101111001011001010110000101101101011010'B
- Constraint:
car_UplinkDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 00 05 54 55 54 57 56 21 0c 51 50 53 52 5d 5c 5f 5e 59 58 5b 5a

- No.: 1932
- Timestamp: 17:17:41:597_0
- RFN: 6030
- Chip: 14336
- Event: Send
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_REQ
- Source: ts_SS_DownloadSecurityKey:lt_DownloadKeyCRLC LINE 1
- Message Structure:
CRLC_SecurityMode_Config_REQ
. (IntegerType)cellId[-1] = -1
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity[0] = 0
. . (BitStringType)startValue[20] = "00000000000000000000"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = '01010111010101100101000101010000010100110101001001011101010111000101111101011110010110010101100001011011010110100101010101010100'B
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CRLC_SecurityModeCfgReq
- BinaryMessage:
30 21 02 01 ff 30 1c 0a 01 00 03 04 04 00 00 00 03 11 00 57 56 51 50 53 52 5d 5c 5f 5e 59 58 5b 5a 55 54

- No.: 1933
- Timestamp: 17:17:41:597_1
- RFN: 6030
- Chip: 16128
- Event: Receive
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_CNF
- Source: ts_SS_DownloadSecurityKey:lt_DownloadKeyCRLC LINE 2
- Message Structure:
CRLC_SecurityMode_Config_CNF
. (IntegerType)cellId[0] = -1
- Constraint:
ca_CRLC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1940
- Timestamp: 17:17:41:598_3
- RFN: 6030
- Chip: 20480
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 1
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 0
. (IntegerType)count_I_LSB_UL[-1] = -
. (IntegerType)count_I_LSB_DL[-1] = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 00 02 01 00 02 01 00

- No.: 1941
- Timestamp: 17:17:41:599_0
- RFN: 6030
- Chip: 22016
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 2
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 0
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 00 02 01 00

- No.: 1942
- Timestamp: 17:17:41:599_1
- RFN: 6030
- Chip: 23808
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 3
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 1
. (IntegerType)count_I_LSB_UL[-1] = -
. (IntegerType)count_I_LSB_DL[-1] = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 01 02 01 00

- No.: 1943
- Timestamp: 17:17:41:599_2
- RFN: 6030
- Chip: 25344
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 4
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 1
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 1944
- Timestamp: 17:17:41:600_0
- RFN: 6030
- Chip: 27392
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 5
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 2
. (IntegerType)count_I_LSB_UL[-1] = -
. (IntegerType)count_I_LSB_DL[-1] = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 02 02 01 00

- No.: 1945
- Timestamp: 17:17:41:600_1
- RFN: 6030
- Chip: 28928
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 6
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 2
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 1946
- Timestamp: 17:17:41:601_0
- RFN: 6030
- Chip: 30976
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 7
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 3
. (IntegerType)count_I_LSB_UL[-1] = -
. (IntegerType)count_I_LSB_DL[-1] = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 03 02 01 00

- No.: 1947
- Timestamp: 17:17:41:601_1
- RFN: 6030
- Chip: 32768
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 8
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 3
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 1948
- Timestamp: 17:17:41:602_0
- RFN: 6030
- Chip: 34560
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 9
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 4
. (IntegerType)count_I_LSB_UL[-1] = -
. (IntegerType)count_I_LSB_DL[-1] = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 04 02 01 00

- No.: 1949
- Timestamp: 17:17:41:602_1
- RFN: 6030
- Chip: 36096
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 10
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 4
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 1953
- Timestamp: 17:17:41:603_2
- RFN: 6031
- Chip: 1280
- Event: Send
- PCO: CRLC
- Message: CRLC_Integrity_Activate_REQ
- Source: ts_CRLC_DL_Integrity LINE 1
- Message Structure:
CRLC_Integrity_Activate_REQ
. (IntegerType)cellId[-1] = -1
. (CN_DomainIdentity)cn_DomainIdentity[0] = 0
. IntegrityActivationInfo
. . IntegrityProtectionModeInfo
. . . IntegrityProtectionModeCommand
. . . . startIntegrityProtection
. . . . . (BitStringType)integrityProtInitNumber[32] = "00000000000000000000000000000001"
. . . (IntegrityProtectionAlgorithm)integrityProtectionAlgorithm[0] = 0
- Constraint:
ca_CRLC_DL_IntegrityActivateReq
- BinaryMessage:
30 14 02 01 ff 0a 01 00 30 0c 30 07 03 05 00 00 00 00 01 0a 01 00

- No.: 1954
- Timestamp: 17:17:41:604_0
- RFN: 6031
- Chip: 3072
- Event: Receive
- PCO: CRLC
- Message: CRLC_Integrity_Activate_CNF
- Source: ts_CRLC_DL_Integrity LINE 2
- Message Structure:
CRLC_Integrity_Activate_CNF
. (IntegerType)cellId[0] = -1
- Constraint:
ca_CRLC_IntegrityActivateCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1961
- Timestamp: 17:17:41:605_0
- RFN: 6031
- Chip: 7936
- Event: Send
- PCO: CRLC
- Message: CRLC_Integrity_Activate_REQ
- Source: ts_RB2_UL_IntegrityActivate LINE 1
- Message Structure:
CRLC_Integrity_Activate_REQ
. (IntegerType)cellId[-1] = -1
. (CN_DomainIdentity)cn_DomainIdentity[0] = 0
. IntegrityActivationInfo
. . IntegrityProtActivationInfoList
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity[-1] = 2
. . . . (IntegerType)rrc_MessageSequenceNumber[-1] = 0
- Constraint:
ca_CRLC_UL_IntegrityActivateReq
- BinaryMessage:
30 10 02 01 ff 0a 01 00 30 08 30 06 02 01 02 02 01 00

- No.: 1962
- Timestamp: 17:17:41:605_1
- RFN: 6031
- Chip: 9472
- Event: Receive
- PCO: CRLC
- Message: CRLC_Integrity_Activate_CNF
- Source: ts_RB2_UL_IntegrityActivate LINE 2
- Message Structure:
CRLC_Integrity_Activate_CNF
. (IntegerType)cellId[0] = -1
- Constraint:
ca_CRLC_IntegrityActivateCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1969
- Timestamp: 17:17:41:607_0
- RFN: 6031
- Chip: 16128
- Event: Send
- PCO: AM
- Message: RLC_AM_DATA_REQ
- Source: ts_RRC_Security:lt_SendSecurityModeCommand LINE 16
- Message Structure:
RLC_AM_DATA_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 2
. AmConfirmationRequest
. aM_message
. . DL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00000000000000000000000000000000"
. . . . (IntegerType)rrc_MessageSequenceNumber[-1] = 0
. . . DL_DCCH_MessageType
. . . . SecurityModeCommand
. . . . . r3
. . . . . . SecurityModeCommand_r3_IEs
. . . . . . . (IntegerType)rrc_TransactionIdentifier[-1] = 0
. . . . . . . SecurityCapability
. . . . . . . . (BitStringType)cipheringAlgorithmCap[16] = '0000000000000011'B
. . . . . . . . (BitStringType)integrityProtectionAlgorithmCap[16] = '0000000000000010'B
. . . . . . . CipheringModeInfo
. . . . . . . IntegrityProtectionModeInfo
. . . . . . . . IntegrityProtectionModeCommand
. . . . . . . . . startIntegrityProtection
. . . . . . . . . . (BitStringType)integrityProtInitNumber[32] = "00000000000000000000000000000001"
. . . . . . . . (IntegrityProtectionAlgorithm)integrityProtectionAlgorithm[0] = 0
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity[0] = 0
. . . . . . . InterRAT_UE_SecurityCapList
. . . . . . laterNonCriticalExtensions
- Constraint:
cas_RRC_SecModeCmd
- BinaryMessage:
30 17 02 01 ff 02 01 02 05 00 80 00 00 00 04 04 00 01 80 01 40 00 00 00 20

- No.: 1978
- Timestamp: 17:17:41:731_0
- RFN: 6043
- Chip: 30976
- Event: Receive
- PCO: AM
- Message: RLC_AM_DATA_IND
- Source: ts_RRC_Security:lt_StartSecurity_UE LINE 8
- Message Structure:
RLC_AM_DATA_IND
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 2
. IntegrityResult
. . (IntegrityStatus)integrityUsed[0] = 0
. aM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "10000001100000001110110111011101"
. . . . (IntegerType)rrc_MessageSequenceNumber[4] = 1
. . . UL_DCCH_MessageType
. . . . SecurityModeComplete
. . . . . (IntegerType)rrc_TransactionIdentifier[2] = 0
. . . . . IntegrityProtActivationInfo
. . . . . . RRC_MessageSequenceNumberList
. . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . (IntegerType)_elem[4] = 0
. . . . . laterNonCriticalExtensions
- Constraint:
car_RRC_SecModeCmpl
- BinaryMessage:
30 12 02 01 ff 02 01 02 0a 01 00 c0 c0 76 ee 8d 21 00 00 00

- No.: 1979
- Timestamp: 17:17:41:732_0
- RFN: 6043
- Chip: 32512
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_Security:lt_StartSecurity_UE LINE 8
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1981
- Timestamp: 17:17:41:733_0
- RFN: 6043
- Chip: 35584
- Event: Send
- PCO: CRLC
- Message: CRLC_Integrity_Activate_REQ
- Source: ts_CRLC_UL_Integrity LINE 1
- Message Structure:
CRLC_Integrity_Activate_REQ
. (IntegerType)cellId[-1] = -1
. (CN_DomainIdentity)cn_DomainIdentity[0] = 0
. IntegrityActivationInfo
. . IntegrityProtActivationInfoList
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity[-1] = 0
. . . . (IntegerType)rrc_MessageSequenceNumber[-1] = 0
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity[-1] = 1
. . . . (IntegerType)rrc_MessageSequenceNumber[-1] = 0
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity[-1] = 3
. . . . (IntegerType)rrc_MessageSequenceNumber[-1] = 0
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity[-1] = 4
. . . . (IntegerType)rrc_MessageSequenceNumber[-1] = 0
- Constraint:
ca_CRLC_UL_IntegrityActivateReq
- BinaryMessage:
30 28 02 01 ff 0a 01 00 30 20 30 06 02 01 00 02 01 00 30 06 02 01 01 02 01 00 30 06 02 01 03 02 01 00 30 06 02 01 04 02 01 00

- No.: 1982
- Timestamp: 17:17:41:733_1
- RFN: 6043
- Chip: 37632
- Event: Receive
- PCO: CRLC
- Message: CRLC_Integrity_Activate_CNF
- Source: ts_CRLC_UL_Integrity LINE 2
- Message Structure:
CRLC_Integrity_Activate_CNF
. (IntegerType)cellId[0] = -1
- Constraint:
ca_CRLC_IntegrityActivateCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1987
- Timestamp: 17:17:41:734_2
- RFN: 6044
- Chip: 3840
- Event: Send
- PCO: Dc
- Message: RRC_DataReq
- Source: ts_GMM_TriggerPSRegistrationAtSwitchOn_NMO_I LINE 9
- Message Structure:
RRC_DataReq
. (IntegerType)cellId[-1] = -1
. (SS_RB_Identity)rB_Id[-1] = 3
. (LogicChGERAN)ch[-1] = -
. (SapId)sapId[1] = -
. (SS_CN_DomainIdentity)cN_Domain[-1] = 0
. LOCATIONUPDATINGACCEPT
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)mMProtocolDiscriminator[4] = '0101'B
. . (MsgType)msgType[8] = '00000010'B
. . LocAreaId_v
. . . (OctetStringType)plmn[3] = '00F110'O
. . . (OctetStringType)lac[2] = '0001'O
. . MM_MS_Identity
. . . (IEI8)iei[8] = '00010111'B
. . . (Length)iel[1] = '05'O
. . . (B4)iDigit1[4] = '1111'B
. . . (B1)oddEvenInd[1] = '0'B
. . . (B3)typeOfId[3] = '100'B
. . . (OctetStringType)otherDigits[-1] = '12345678'O
. . (FollowOnProceed)followOnProceed[8] = '10100001'B
. . (CTSPerm)cTSPerm[8] = '10100010'B
. . PLMN_List
- Constraint:
ca_DataReq
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 00 05 02 00 f1 10 00 01 17 05 f4 12 34 56 78 a1 a2

- No.: 1994
- Timestamp: 17:17:41:871_0
- RFN: 6057
- Chip: 29952
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_GMM_TriggerPSRegistrationAtSwitchOn_NMO_I LINE 10
- Message Structure:
RRC_DataInd
. (IntegerType)cellId[0] = -1
. (SS_RB_Identity)rB_Id[0] = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain[0] = 0
. (START_Value)start[0] = -
. TMSIREALLOCATIONCOMPLETE
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)mMProtocolDiscriminator[4] = '0101'B
. . (MsgType)msgType[8] = '10011011'B
- Constraint:
car_UplinkDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 00 05 9b

- No.: 2004
- Timestamp: 17:17:41:872_4
- RFN: 6057
- Chip: 35328
- Event: Start Timer
- Source: ts_RRC_Delay LINE 1
- Message Structure:
no details available
- Constraint:
t_Dly (1000 Ms)
- BinaryMessage:

- No.: 2008
- Timestamp: 17:17:42:872_0
- RFN: 6157
- Chip: 35072
- Event: Timeout
- Source: ts_RRC_Delay LINE 2
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 2013
- Timestamp: 17:17:42:873_0
- RFN: 6158
- Chip: 1536
- Event: Send
- PCO: UM
- Message: RLC_UM_DATA_REQ
- Source: ts_RRC_ConnRel:lt_Send_RRC_ConnectionRelease LINE 3
- Message Structure:
RLC_UM_DATA_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 1
. uM_message
. . DL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00000000000000000000000000000000"
. . . . (IntegerType)rrc_MessageSequenceNumber[-1] = 0
. . . DL_DCCH_MessageType
. . . . RRCConnectionRelease
. . . . . r3
. . . . . . RRCConnectionRelease_r3_IEs
. . . . . . . (IntegerType)rrc_TransactionIdentifier[-1] = 0
. . . . . . . (IntegerType)n_308[-1] = 1
. . . . . . . (ReleaseCause)releaseCause[0] = 0
. . . . . . . Rplmn_Information
. . . . . . laterNonCriticalExtensions
. (BooleanType)specialLI = FALSE
- Constraint:
cas_RRC_ConnRelDCCH
- BinaryMessage:
30 10 02 01 ff 02 01 01 80 00 00 00 03 c8 00 01 01 00

- No.: 2017
- Timestamp: 17:17:43:001_0
- RFN: 6170
- Chip: 29440
- Event: Receive
- PCO: UM
- Message: RLC_UM_DATA_IND
- Source: ts_RRC_ConnRel:lt_Send_RRC_ConnectionRelease LINE 4
- Message Structure:
RLC_UM_DATA_IND
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 1
. IntegrityResult
. uM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "10101101101011101001000000111001"
. . . . (IntegerType)rrc_MessageSequenceNumber[4] = 1
. . . UL_DCCH_MessageType
. . . . RRCConnectionReleaseComplete
. . . . . (IntegerType)rrc_TransactionIdentifier[2] = 0
. . . . . FailureCauseWithProtErr
. . . . . laterNonCriticalExtensions
- Constraint:
car_RRC_ConnRelCmplUM
- BinaryMessage:
30 0e 02 01 ff 02 01 01 05 00 d6 d7 48 1c 8c 40

- No.: 2018
- Timestamp: 17:17:43:001_1
- RFN: 6170
- Chip: 30720
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ConnRel:lt_Send_RRC_ConnectionRelease LINE 4
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2021
- Timestamp: 17:17:43:002_1
- RFN: 6170
- Chip: 32768
- Event: Start Timer
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 1
- Message Structure:
no details available
- Constraint:
t_Dly (5000 Ms)
- BinaryMessage:

- No.: 2025
- Timestamp: 17:17:43:160_0
- RFN: 6186
- Chip: 29184
- Event: Receive
- PCO: UM
- Message: RLC_UM_DATA_IND
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 4
- Message Structure:
RLC_UM_DATA_IND
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 1
. IntegrityResult
. uM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00011100010101000111110101101001"
. . . . (IntegerType)rrc_MessageSequenceNumber[4] = 2
. . . UL_DCCH_MessageType
. . . . RRCConnectionReleaseComplete
. . . . . (IntegerType)rrc_TransactionIdentifier[2] = 0
. . . . . FailureCauseWithProtErr
. . . . . laterNonCriticalExtensions
- Constraint:
car_RRC_ConnRelCmplUM
- BinaryMessage:
30 0e 02 01 ff 02 01 01 05 00 8e 2a 3e b4 94 40

- No.: 2026
- Timestamp: 17:17:43:161_0
- RFN: 6186
- Chip: 32256
- Event: Cancel Timer
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 4
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 2027
- Timestamp: 17:17:43:161_1
- RFN: 6186
- Chip: 32768
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 4
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2033
- Timestamp: 17:17:43:163_0
- RFN: 6186
- Chip: 37888
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 1
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 01 0a 01 00 05 00

- No.: 2037
- Timestamp: 17:17:43:168_0
- RFN: 6187
- Chip: 21760
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 2040
- Timestamp: 17:17:43:169_2
- RFN: 6187
- Chip: 25344
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 2
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 02 0a 01 00 05 00

- No.: 2044
- Timestamp: 17:17:43:173_0
- RFN: 6188
- Chip: 2816
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 2047
- Timestamp: 17:17:43:174_2
- RFN: 6188
- Chip: 6400
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 3
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 03 0a 01 00 05 00

- No.: 2051
- Timestamp: 17:17:43:179_0
- RFN: 6188
- Chip: 24320
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 3
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 2054
- Timestamp: 17:17:43:180_0
- RFN: 6188
- Chip: 27904
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 4
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 04 0a 01 00 05 00

- No.: 2058
- Timestamp: 17:17:43:187_0
- RFN: 6189
- Chip: 15872
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 4
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 2061
- Timestamp: 17:17:43:188_0
- RFN: 6189
- Chip: 22528
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 1
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 136
. . . . . UL_RLC_Mode
. . . . . . UL_UM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (NoExplicitDiscard)timerBasedNoExplicit[0] = 9
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 1
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 1
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_UM_Info
- BinaryMessage:
30 22 02 01 ff 02 01 01 0a 01 00 30 17 30 0d 05 00 30 09 02 02 00 88 30 03 0a 01 09 30 06 02 01 01 02 01 01

- No.: 2065
- Timestamp: 17:17:43:193_0
- RFN: 6190
- Chip: 0
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 2066
- Timestamp: 17:17:43:195_0
- RFN: 6190
- Chip: 7424
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 3
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 2
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 2
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 2
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 02 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 13 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 02 02 01 02

- No.: 2070
- Timestamp: 17:17:43:202_0
- RFN: 6190
- Chip: 37120
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 4
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 2071
- Timestamp: 17:17:43:204_0
- RFN: 6191
- Chip: 5632
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 5
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 3
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 3
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 3
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 03 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 13 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 03 02 01 03

- No.: 2075
- Timestamp: 17:17:43:213_0
- RFN: 6192
- Chip: 768
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 6
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 3
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 2076
- Timestamp: 17:17:43:215_0
- RFN: 6192
- Chip: 7936
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 7
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 4
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 4
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 4
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 04 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 13 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 04 02 01 04

- No.: 2080
- Timestamp: 17:17:43:223_0
- RFN: 6193
- Chip: 256
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 8
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 4
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 2103
- Timestamp: 17:17:43:225_6
- RFN: 6193
- Chip: 11520
- Event: Start Timer
- Source: ts_GMM_TriggerPSRegistrationAtSwitchOn_NMO_I LINE 12
- Message Structure:
no details available
- Constraint:
t_WaitS (1 Sec)
- BinaryMessage:

- No.: 2110
- Timestamp: 17:17:44:232_0
- RFN: 6293
- Chip: 33024
- Event: Timeout
- Source: ts_GMM_TriggerPSRegistrationAtSwitchOn_NMO_I LINE 13
- Message Structure:
no details available
- Constraint:
t_WaitS
- BinaryMessage:

- No.: 2112
- Timestamp: 17:17:44:232_2
- RFN: 6293
- Chip: 35584
- Event: Send
- PCO: Ut
- Message: AT_CmdReq
- Source: ts_AT_TriggerGMM_Attach LINE 1
- Message Structure:
AT_CmdReq
. (IA5StringType)cmd[-1] = "AT+CGATT=1"
. (HexStringType)sMS_BlockMode[-1] = -
- Constraint:
ca_AT_CmdReq
- BinaryMessage:
41 54 2b 43 47 41 54 54 3d 31 3c 43 52 3e

- No.: 2116
- Timestamp: 17:17:47:156_0
- RFN: 6586
- Chip: 14080
- Event: Receive
- PCO: Ut
- Message: AT_CmdCnf
- Source: ts_AT_TriggerGMM_Attach LINE 2
- Message Structure:
AT_CmdCnf
. (BooleanType)result = TRUE
. (IA5StringType)resultString[18] = "OK"
. (HexStringType)sMS_BlockMode[0] = -
- Constraint:
ca_AT_CmdCnf
- BinaryMessage:
80 3c 43 52 3e 3c 4c 46 3e 4f 4b 3c 43 52 3e 3c 4c 46 3e

- No.: 2133
- Timestamp: 17:17:47:159_0
- RFN: 6586
- Chip: 23040
- Event: Receive
- PCO: CPHY
- Message: CPHY_Out_of_Sync_IND
- Source: RRC_DefConnEst LINE 7
- Message Structure:
CPHY_Out_of_Sync_IND
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 20
- Constraint:
ca_OutOfSyncInd
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 2134
- Timestamp: 17:17:47:159_1
- RFN: 6586
- Chip: 23808
- Event: Cancel Timer
- Source: RRC_DefConnEst LINE 7
- Message Structure:
no details available
- Constraint:
t_T312
- BinaryMessage:

- No.: 2135
- Timestamp: 17:17:47:159_2
- RFN: 6586
- Chip: 24320
- Event: Default
- Source: RRC_DefConnEst LINE 0
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2136
- Timestamp: 17:17:47:159_3
- RFN: 6586
- Chip: 24832
- Event: Default
- Source: ts_RRC_ConnEst:lt_RcvConnReq LINE 2
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2141
- Timestamp: 17:17:49:688_0
- RFN: 6839
- Chip: 23040
- Event: Receive
- PCO: TM
- Message: RLC_TR_DATA_IND
- Source: ts_RRC_ConnEst:lt_RcvConnReq LINE 2
- Message Structure:
RLC_TR_DATA_IND
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 0
. tM_message
. . UL_CCCH_Message
. . . IntegrityCheckInfo
. . . UL_CCCH_MessageType
. . . . RRCConnectionRequest
. . . . . InitialUE_Identity
. . . . . . TMSI_and_LAI_GSM_MAP
. . . . . . . (BitStringType)tmsi[32] = "00010010001101000101011001111000"
. . . . . . . LAI
. . . . . . . . PLMN_Identity
. . . . . . . . . MCC
. . . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . . (IntegerType)_elem[4] = 1
. . . . . . . . . MNC
. . . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . . (IntegerType)_elem[4] = 1
. . . . . . . . (BitStringType)lac[16] = '0000000000000001'B
. . . . . (EstablishmentCause)establishmentCause[5] = 12
. . . . . (ProtocolErrorIndicator)protocolErrorIndicator[1] = 0
. . . . . MeasuredResultsOnRACH
. . . . . v3d0NonCriticalExtensions
- Constraint:
car_RRC_ConnReq
- BinaryMessage:
30 11 02 01 00 02 01 00 21 12 34 56 78 00 10 08 00 0b 00

- No.: 2145
- Timestamp: 17:17:49:699_0
- RFN: 6840
- Chip: 25344
- Event: Send
- PCO: UM
- Message: RLC_UM_DATA_REQ
- Source: ts_RRC_ConnEst:lt_Send_ConnSetUp LINE 22
- Message Structure:
RLC_UM_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 0
. uM_message
. . DL_CCCH_Message
. . . IntegrityCheckInfo
. . . DL_CCCH_MessageType
. . . . RRCConnectionSetup
. . . . . r3
. . . . . . RRCConnectionSetup_r3_IEs
. . . . . . . InitialUE_Identity
. . . . . . . . TMSI_and_LAI_GSM_MAP
. . . . . . . . . (BitStringType)tmsi[32] = "00010010001101000101011001111000"
. . . . . . . . . LAI
. . . . . . . . . . PLMN_Identity
. . . . . . . . . . . MCC
. . . . . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . . . . (IntegerType)_elem[4] = 1
. . . . . . . . . . . MNC
. . . . . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . . . . (IntegerType)_elem[4] = 1
. . . . . . . . . . (BitStringType)lac[16] = '0000000000000001'B
. . . . . . . (IntegerType)rrc_TransactionIdentifier[-1] = 0
. . . . . . . (IntegerType)activationTime[-1] = -
. . . . . . . U_RNTI
. . . . . . . . (BitStringType)srnc_Identity[12] = "000000000001"
. . . . . . . . (BitStringType)s_RNTI[20] = "00000000000000000001"
. . . . . . . (BitStringType)new_c_RNTI[16] = -
. . . . . . . (RRC_StateIndicator)rrc_StateIndicator[0] = 0
. . . . . . . (IntegerType)utran_DRX_CycleLengthCoeff[-1] = 9
. . . . . . . CapabilityUpdateRequirement
. . . . . . . . (BooleanType)ue_RadioCapabilityFDDUpdateRequirement = TRUE
. . . . . . . . (BooleanType)ue_RadioCapabilityTDDUpdateRequirement = FALSE
. . . . . . . . SystemSpecificCapUpdateReqList
. . . . . . . . . (SystemSpecificCapUpdateReq)_elem[0] = 0
. . . . . . . SRB_InformationSetupList2
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity[-1] = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_UM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 1
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex[-1] = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 1
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity[-1] = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 2
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 2
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 2
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 2
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex[-1] = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 2
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 2
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity[-1] = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 3
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 3
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 3
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 3
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex[-1] = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 3
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 3
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity[-1] = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 4
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 4
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 4
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 4
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex[-1] = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 4
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 4
. . . . . . . UL_CommonTransChInfo
. . . . . . . . TFC_Subset
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . TFCS
. . . . . . . . . . . ExplicitTFCS_Configuration
. . . . . . . . . . . . TFCS_ReconfAdd
. . . . . . . . . . . . . ctfcSize
. . . . . . . . . . . . . . ctfc2Bit
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . . . . . . . (IntegerType)ctfc2[-1] = 0
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . . . . . . . (IntegerType)ctfc2[-1] = 1
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC[-1] = 11
. . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaD[-1] = 15
. . . . . . . . . . . . . . . . . . . (IntegerType)referenceTFC_ID[-1] = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . UL_AddReconfTransChInfoList
. . . . . . . . UL_AddReconfTransChInformation
. . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType[0] = 0
. . . . . . . . . (IntegerType)transportChannelIdentity[-1] = 5
. . . . . . . . . TransportFormatSet
. . . . . . . . . . DedicatedTransChTFS
. . . . . . . . . . . tti
. . . . . . . . . . . . DedicatedDynamicTF_InfoList
. . . . . . . . . . . . . DedicatedDynamicTF_Info
. . . . . . . . . . . . . . rlc_Size
. . . . . . . . . . . . . . . BitModeRLC_SizeInfo
. . . . . . . . . . . . . . . . sizeType2
. . . . . . . . . . . . . . . . . (IntegerType)part1[-1] = 2
. . . . . . . . . . . . . . . . . (IntegerType)part2[-1] = -
. . . . . . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . LogicalChannelList
. . . . . . . . . . . SemistaticTF_Information
. . . . . . . . . . . . ChannelCodingType
. . . . . . . . . . . . . (CodingRate)convolutional[0] = 1
. . . . . . . . . . . . (IntegerType)rateMatchingAttribute[-1] = 192
. . . . . . . . . . . . (CRC_Size)crc_Size[0] = 3
. . . . . . . DL_CommonTransChInfo
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . dl_Parameters
. . . . . . . DL_AddReconfTransChInfoList
. . . . . . . . DL_AddReconfTransChInformation
. . . . . . . . . (DL_TrCH_Type)dl_TransportChannelType[0] = 0
. . . . . . . . . (IntegerType)dl_transportChannelIdentity[-1] = 10
. . . . . . . . . tfs_SignallingMode
. . . . . . . . . . UL_TransportChannelIdentity
. . . . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType[0] = 0
. . . . . . . . . . . (IntegerType)ul_TransportChannelIdentity[-1] = 5
. . . . . . . . . QualityTarget
. . . . . . . . . . (IntegerType)bler_QualityValue[-1] = -20
. . . . . . . . . TM_SignallingInfo
. . . . . . . FrequencyInfo
. . . . . . . (IntegerType)maxAllowedUL_TX_Power[-1] = -
. . . . . . . UL_ChannelRequirement
. . . . . . . . UL_DPCH_Info
. . . . . . . . . UL_DPCH_PowerControlInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (IntegerType)dpcch_PowerOffset[-1] = -40
. . . . . . . . . . . (IntegerType)pc_Preamble[-1] = 1
. . . . . . . . . . . (IntegerType)sRB_delay[-1] = 7
. . . . . . . . . . . PowerControlAlgorithm
. . . . . . . . . . . . (IntegerType)algorithm1[-1] = 1
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (ScramblingCodeType)scramblingCodeType[0] = 1
. . . . . . . . . . . (IntegerType)scramblingCode[-1] = 0
. . . . . . . . . . . (IntegerType)numberOfDPDCH[-1] = -
. . . . . . . . . . . (SpreadingFactor)spreadingFactor[0] = 4
. . . . . . . . . . . (BooleanType)tfci_Existence = TRUE
. . . . . . . . . . . (IntegerType)numberOfFBI_Bits[-1] = -
. . . . . . . . . . . (PuncturingLimit)puncturingLimit[0] = 15
. . . . . . . DL_CommonInformation
. . . . . . . . DL_DPCH_InfoCommon
. . . . . . . . . cfnHandling
. . . . . . . . . . initialise
. . . . . . . . . . . (IntegerType)cfntargetsfnframeoffset[-1] = -
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . DL_DPCH_PowerControlInfo
. . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . (DPC_Mode)dpc_Mode[0] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPilot_pdpdch[-1] = 0
. . . . . . . . . . . Dl_rate_matching_restriction
. . . . . . . . . . . SF512_AndPilot
. . . . . . . . . . . . (PilotBits128)sfd128[0] = 0
. . . . . . . . . . . (PositionFixedOrFlexible)positionFixedOrFlexible[0] = 0
. . . . . . . . . . . (BooleanType)tfci_Existence = FALSE
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . (IntegerType)defaultDPCH_OffsetValue[-1] = 459
. . . . . . . . . . DPCH_CompressedModeInfo
. . . . . . . . . . (TX_DiversityMode)tx_DiversityMode[0] = 0
. . . . . . . . . . SSDT_Information
. . . . . . . DL_InformationPerRL_List
. . . . . . . . DL_InformationPerRL
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . PrimaryCPICH_Info
. . . . . . . . . . . . (IntegerType)primaryScramblingCode[-1] = 100
. . . . . . . . . . . PDSCH_SHO_DCH_Info
. . . . . . . . . . . PDSCH_CodeMapping
. . . . . . . . . DL_DPCH_InfoPerRL
. . . . . . . . . . fdd
. . . . . . . . . . . (PCPICH_UsageForChannelEst)pCPICH_UsageForChannelEst[0] = 0
. . . . . . . . . . . (IntegerType)dpch_FrameOffset[-1] = 18
. . . . . . . . . . . SecondaryCPICH_Info
. . . . . . . . . . . DL_ChannelisationCodeList
. . . . . . . . . . . . DL_ChannelisationCode
. . . . . . . . . . . . . (IntegerType)secondaryScramblingCode[-1] = 1
. . . . . . . . . . . . . SF512_AndCodeNumber
. . . . . . . . . . . . . . (IntegerType)sf128[-1] = 0
. . . . . . . . . . . . . (ScramblingCodeChange)scramblingCodeChange[0] = 1
. . . . . . . . . . . (IntegerType)tpc_CombinationIndex[-1] = 0
. . . . . . . . . . . (SSDT_CellIdentity)ssdt_CellIdentity[0] = -
. . . . . . . . . . . (ClosedLoopTimingAdjMode)closedLoopTimingAdjMode[0] = -
. . . . . . . . . SCCPCH_InfoForFACH
. . . . . . laterNonCriticalExtensions
. (BooleanType)specialLI = TRUE
- Constraint:
cas_RRC_ConnSetup
- BinaryMessage:
30 78 02 01 00 02 01 00 30 e7 22 46 8a cf 00 02 01 00 01 00 04 00 00 4d 82 69 3a 10 10 89 0d 42 00 02 81 9e 8e 46 c9 a6 7c 9c 4e 74 20 a5 12 3a 8c 00 15 13 3d 1c 8d 93 4c f9 38 9c e8 42 52 24 b5 28 00 4a 46 7a 39 1b 26 99 f2 71 39 d0 86 b4 49 ea 70 00 d4 c8 00 06 25 2b f0 02 00 08 82 23 bf 66 08 98 95 a5 47 a2 00 00 01 3f 90 0a 14 e5 82 06 40 09 0c 28 08 01 01 ff

- No.: 2166
- Timestamp: 17:17:49:721_6
- RFN: 6842
- Chip: 35072
- Event: Start Timer
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 3
- Message Structure:
no details available
- Constraint:
t_WaitMS (13500 Ms)
- BinaryMessage:

- No.: 2173
- Timestamp: 17:17:49:920_1
- RFN: 6862
- Chip: 27904
- Event: Receive
- PCO: CPHY
- Message: CPHY_Sync_IND
- Source: RRC_DefConnEst LINE 5
- Message Structure:
CPHY_Sync_IND
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 20
- Constraint:
ca_SyncInd
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 2174
- Timestamp: 17:17:49:920_2
- RFN: 6862
- Chip: 28928
- Event: Cancel Timer
- Source: RRC_DefConnEst LINE 5
- Message Structure:
no details available
- Constraint:
t_T312
- BinaryMessage:

- No.: 2175
- Timestamp: 17:17:49:920_3
- RFN: 6862
- Chip: 29440
- Event: Default
- Source: RRC_DefConnEst LINE 0
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2176
- Timestamp: 17:17:49:920_4
- RFN: 6862
- Chip: 29696
- Event: Default
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2183
- Timestamp: 17:17:50:021_0
- RFN: 6872
- Chip: 34816
- Event: Receive
- PCO: AM
- Message: RLC_AM_DATA_IND
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
RLC_AM_DATA_IND
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 2
. IntegrityResult
. . (IntegrityStatus)integrityUsed[0] = 4294967296
. aM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . UL_DCCH_MessageType
. . . . RRCConnectionSetupComplete
. . . . . (IntegerType)rrc_TransactionIdentifier[2] = 0
. . . . . STARTList
. . . . . . STARTSingle
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity[1] = 1
. . . . . . . (BitStringType)start_Value[20] = "00000000000000000010"
. . . . . . STARTSingle
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity[1] = 0
. . . . . . . (BitStringType)start_Value[20] = "00000000000000000010"
. . . . . UE_RadioAccessCapability
. . . . . . (AccessStratumReleaseIndicator)accessStratumReleaseIndicator[0] = 0
. . . . . . PDCP_Capability
. . . . . . . (BooleanType)losslessSRNS_RelocationSupport = FALSE
. . . . . . . supportForRfc2507
. . . . . . . . (MaxHcContextSpace)supported[3] = 4
. . . . . . RLC_Capability
. . . . . . . (TotalRLC_AM_BufferSize)totalRLC_AM_BufferSize[3] = 2
. . . . . . . (MaximumRLC_WindowSize)maximumRLC_WindowSize[1] = 0
. . . . . . . (MaximumAM_EntityNumberRLC_Cap)maximumAM_EntityNumber[3] = 3
. . . . . . TransportChannelCapability
. . . . . . . DL_TransChCapability
. . . . . . . . (MaxNoBits)maxNoBitsReceived[4] = 7
. . . . . . . . (MaxNoBits)maxConvCodeBitsReceived[4] = 1
. . . . . . . . TurboSupport
. . . . . . . . . (MaxNoBits)supported[4] = 7
. . . . . . . . (MaxSimultaneousTransChsDL)maxSimultaneousTransChs[2] = 1
. . . . . . . . (IntegerType)maxSimultaneousCCTrCH_Count[3] = 1
. . . . . . . . (MaxTransportBlocksDL)maxReceivedTransportBlocks[4] = 3
. . . . . . . . (MaxNumberOfTFC_DL)maxNumberOfTFC[4] = 5
. . . . . . . . (MaxNumberOfTF)maxNumberOfTF[3] = 1
. . . . . . . UL_TransChCapability
. . . . . . . . (MaxNoBits)maxNoBitsTransmitted[4] = 3
. . . . . . . . (MaxNoBits)maxConvCodeBitsTransmitted[4] = 1
. . . . . . . . TurboSupport
. . . . . . . . . (MaxNoBits)supported[4] = 3
. . . . . . . . (MaxSimultaneousTransChsUL)maxSimultaneousTransChs[3] = 2
. . . . . . . . modeSpecificInfo
. . . . . . . . (MaxTransportBlocksUL)maxTransmittedBlocks[4] = 4
. . . . . . . . (MaxNumberOfTFC_UL)maxNumberOfTFC[4] = 5
. . . . . . . . (MaxNumberOfTF)maxNumberOfTF[3] = 0
. . . . . . RF_Capability
. . . . . . . fddRF_Capability
. . . . . . . . (IntegerType)ue_PowerClass[2] = 4
. . . . . . . . (TxRxFrequencySeparation)txRxFrequencySeparation[2] = 0
. . . . . . . tddRF_Capability
. . . . . . PhysicalChannelCapability
. . . . . . . fddPhysChCapability
. . . . . . . . DL_PhysChCapabilityFDD
. . . . . . . . . (IntegerType)maxNoDPCH_PDSCH_Codes[3] = 1
. . . . . . . . . (MaxNoPhysChBitsReceived)maxNoPhysChBitsReceived[4] = 6
. . . . . . . . . (BooleanType)supportForSF_512 = FALSE
. . . . . . . . . (BooleanType)supportOfPDSCH = FALSE
. . . . . . . . . SimultaneousSCCPCH_DPCH_Reception
. . . . . . . . UL_PhysChCapabilityFDD
. . . . . . . . . (MaxNoDPDCH_BitsTransmitted)maxNoDPDCH_BitsTransmitted[4] = 3
. . . . . . . . . (BooleanType)supportOfPCPCH = FALSE
. . . . . . . tddPhysChCapability
. . . . . . UE_MultiModeRAT_Capability
. . . . . . . MultiRAT_Capability
. . . . . . . . (BooleanType)supportOfGSM = FALSE
. . . . . . . . (BooleanType)supportOfMulticarrier = FALSE
. . . . . . . (MultiModeCapability)multiModeCapability[2] = 1
. . . . . . SecurityCapability
. . . . . . . (BitStringType)cipheringAlgorithmCap[16] = '0000000000000011'B
. . . . . . . (BitStringType)integrityProtectionAlgorithmCap[16] = '0000000000000010'B
. . . . . . UE_Positioning_Capability
. . . . . . . (BooleanType)standaloneLocMethodsSupported = FALSE
. . . . . . . (BooleanType)ue_BasedOTDOA_Supported = FALSE
. . . . . . . (NetworkAssistedGPS_Supported)networkAssistedGPS_Supported[2] = 3
. . . . . . . (BooleanType)supportForUE_GPS_TimingOfCellFrames = FALSE
. . . . . . . (BooleanType)supportForIPDL = FALSE
. . . . . . MeasurementCapability
. . . . . . . CompressedModeMeasCapability
. . . . . . . . (BooleanType)fdd_Measurements = TRUE
. . . . . . . . (BooleanType)tdd_Measurements = -
. . . . . . . . GSM_Measurements
. . . . . . . . . (BooleanType)gsm900 = TRUE
. . . . . . . . . (BooleanType)dcs1800 = TRUE
. . . . . . . . . (BooleanType)gsm1900 = TRUE
. . . . . . . . (BooleanType)multiCarrierMeasurements = FALSE
. . . . . . . CompressedModeMeasCapability
. . . . . . . . (BooleanType)fdd_Measurements = TRUE
. . . . . . . . (BooleanType)tdd_Measurements = -
. . . . . . . . GSM_Measurements
. . . . . . . . . (BooleanType)gsm900 = TRUE
. . . . . . . . . (BooleanType)dcs1800 = TRUE
. . . . . . . . . (BooleanType)gsm1900 = TRUE
. . . . . . . . (BooleanType)multiCarrierMeasurements = FALSE
. . . . . v370NonCriticalExtensions
- Constraint:
car_RRC_ConnSetupCmpl
- BinaryMessage:
30 27 02 01 ff 02 01 02 0a 05 01 00 00 00 00 4a 0c 00 00 80 00 05 62 37 1b a0 d4 98 cd 11 45 90 60 61 00 03 00 02 31 f9 f8

- No.: 2184
- Timestamp: 17:17:50:023_0
- RFN: 6873
- Chip: 3072
- Event: Cancel Timer
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
t_WaitMS
- BinaryMessage:

- No.: 2185
- Timestamp: 17:17:50:023_1
- RFN: 6873
- Chip: 3328
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2207
- Timestamp: 17:17:50:051_0
- RFN: 6875
- Chip: 33280
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: tc_12_4_1_4c2:lt_Attach_Steps_3To4 LINE 1
- Message Structure:
RRC_DataInd
. (IntegerType)cellId[0] = -1
. (SS_RB_Identity)rB_Id[0] = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain[0] = 1
. (START_Value)start[20] = '00000000000000000010'B
. ATTACHREQUEST
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)gMMProtocolDiscriminator[4] = '1000'B
. . (MsgType)msgType[8] = '00000001'B
. . MS_NetworkCap_lv
. . . (Length)iel[1] = '02'O
. . . (OctetStringType)value[2] = 'E540'O
. . CiphKeySeqNum
. . . (B1)spare1[1] = '0'B
. . . (KeySeq)keySeq[3] = '000'B
. . AttachType
. . . (B1)pre_for[1] = '0'B
. . . (B3)type[3] = '011'B
. . DRXparamter
. . . (B8)splitPGcycleCode[8] = '00000111'B
. . . (B4)cnDRXcoef[4] = '0000'B
. . . (B1)splitOnCCCH[1] = '0'B
. . . (B3)nonDRXtimer[3] = '100'B
. . MS_Identity_lv
. . . (Length)iel[1] = '05'O
. . . (B4)iDigit1[4] = '1111'B
. . . (B1)oddEvenInd[1] = '0'B
. . . (B3)typeOfId[3] = '100'B
. . . (OctetStringType)otherDigits[4] = '12345678'O
. . RAI_v
. . . (OctetStringType)plmn[3] = '00F110'O
. . . (OctetStringType)lac[2] = '0001'O
. . . (OctetStringType)rac[1] = '05'O
. . MSRadioAccessCap_lv
. . . (Length)iel[1] = '0B'O
. . . (OctetStringType)value[11] = '15F38233542A332644A198'O
. . PTMSI_Signature
. . GPRS_Timer
. . . (IEI8)iei[8] = '00010111'B
. . . (B3)unit[3] = '000'B
. . . (B5)value[5] = '10110'B
. . TMSI_Status
- Constraint:
car_PS_InitDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 03 04 04 00 00 20 08 01 02 e5 40 03 07 04 05 f4 12 34 56 78 00 f1 10 00 01 05 0b 15 f3 82 33 54 2a 33 26 44 a1 98 17 16

- No.: 2244
- Timestamp: 17:17:50:057_0
- RFN: 6876
- Chip: 19712
- Event: Send
- PCO: Dc
- Message: RRC_DataReq
- Source: ts_GMM_Authentication LINE 2
- Message Structure:
RRC_DataReq
. (IntegerType)cellId[-1] = -1
. (SS_RB_Identity)rB_Id[-1] = 3
. (LogicChGERAN)ch[-1] = -
. (SapId)sapId[1] = -
. (SS_CN_DomainIdentity)cN_Domain[-1] = 1
. AUTHENTICATIONANDCIPHERINGREQUEST
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)gMMProtocolDiscriminator[4] = '1000'B
. . (MsgType)msgType[8] = '00010010'B
. . IMEISVRequest
. . . (B1)spare1[1] = '0'B
. . . (B3)value[3] = '000'B
. . CiphAlgorithm
. . . (B1)spare1[1] = '0'B
. . . (B3)algorithm[3] = '001'B
. . AC_ReferenceNumber
. . . (B4)value[4] = '0011'B
. . ForceToStandby
. . . (B1)spare[1] = '0'B
. . . (B3)value[3] = '000'B
. . AuthenticationParamterRAND
. . . (IEI8)iei[8] = '00100001'B
. . . (BitStringType)randValue[128] = '01010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101'B
. . CiphKeySeqNum_tv
. . . (IEI4)iei[4] = '1000'B
. . . (B1)spare1[1] = '0'B
. . . (KeySeq)keySeq[3] = '001'B
. . GMM_AUTN
. . . (IEI8)iei[8] = '00101000'B
. . . (Length)iel[1] = '10'O
. . . (BitStringType)aUTN[128] = '01010110010100010101000001010011010100100101110100000000000000000101010101010100010101110101011001010001010100000101001101010010'B
- Constraint:
ca_PS_DataReq
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 08 12 01 30 21 55 55 55 55 55 55 55 55 55 55 55 55 55 55 55 55 81 28 10 56 51 50 53 52 5d 00 00 55 54 57 56 51 50 53 52

- No.: 2248
- Timestamp: 17:17:50:330_0
- RFN: 6903
- Chip: 30976
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_GMM_Authentication LINE 3
- Message Structure:
RRC_DataInd
. (IntegerType)cellId[0] = -1
. (SS_RB_Identity)rB_Id[0] = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain[0] = 1
. (START_Value)start[0] = -
. AUTHENTICATIONANDCIPHERINGRESPONSE
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)gMMProtocolDiscriminator[4] = '1000'B
. . (MsgType)msgType[8] = '00010011'B
. . (B4)spare4[4] = '0000'B
. . AC_ReferenceNumber
. . . (B4)value[4] = '0011'B
. . AuthRsp_tv
. . . (IEI8)iei[8] = '00100010'B
. . . (BitStringType)value[32] = '01010101010101000101011101010110'B
. . GMM_MS_Identity
. . AuthRspExt
. . . (IEI8)iei[8] = '00101001'B
. . . (Length)iel[1] = '0C'O
. . . (BitStringType)rES[96] = '010100010101000001010011010100100101110101011100010111110101111001011001010110000101101101011010'B
- Constraint:
car_PS_UplinkDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 08 13 03 22 55 54 57 56 29 0c 51 50 53 52 5d 5c 5f 5e 59 58 5b 5a

- No.: 2251
- Timestamp: 17:17:50:331_2
- RFN: 6903
- Chip: 33792
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_GMM_Authentication LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2291
- Timestamp: 17:17:50:336_3
- RFN: 6904
- Chip: 15616
- Event: Send
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_REQ
- Source: ts_SS_DownloadSecurityKey:lt_DownloadKeyCRLC LINE 1
- Message Structure:
CRLC_SecurityMode_Config_REQ
. (IntegerType)cellId[-1] = -1
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity[0] = 1
. . (BitStringType)startValue[20] = "00000000000000000000"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = '01010111010101100101000101010000010100110101001001011101010111000101111101011110010110010101100001011011010110100101010101010100'B
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CRLC_SecurityModeCfgReq
- BinaryMessage:
30 21 02 01 ff 30 1c 0a 01 01 03 04 04 00 00 00 03 11 00 57 56 51 50 53 52 5d 5c 5f 5e 59 58 5b 5a 55 54

- No.: 2292
- Timestamp: 17:17:50:337_0
- RFN: 6904
- Chip: 17408
- Event: Receive
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_CNF
- Source: ts_SS_DownloadSecurityKey:lt_DownloadKeyCRLC LINE 2
- Message Structure:
CRLC_SecurityMode_Config_CNF
. (IntegerType)cellId[0] = -1
- Constraint:
ca_CRLC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 2299
- Timestamp: 17:17:50:338_0
- RFN: 6904
- Chip: 21504
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 1
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 0
. (IntegerType)count_I_LSB_UL[-1] = -
. (IntegerType)count_I_LSB_DL[-1] = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 00 02 01 00 02 01 00

- No.: 2300
- Timestamp: 17:17:50:338_1
- RFN: 6904
- Chip: 23296
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 2
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 0
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 00 02 01 00

- No.: 2301
- Timestamp: 17:17:50:339_0
- RFN: 6904
- Chip: 25088
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 3
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 1
. (IntegerType)count_I_LSB_UL[-1] = -
. (IntegerType)count_I_LSB_DL[-1] = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 01 02 01 00

- No.: 2302
- Timestamp: 17:17:50:339_1
- RFN: 6904
- Chip: 26624
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 4
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 1
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 2303
- Timestamp: 17:17:50:340_0
- RFN: 6904
- Chip: 28416
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 5
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 2
. (IntegerType)count_I_LSB_UL[-1] = -
. (IntegerType)count_I_LSB_DL[-1] = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 02 02 01 00

- No.: 2304
- Timestamp: 17:17:50:340_1
- RFN: 6904
- Chip: 29696
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 6
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 2
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 2305
- Timestamp: 17:17:50:340_2
- RFN: 6904
- Chip: 31488
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 7
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 3
. (IntegerType)count_I_LSB_UL[-1] = -
. (IntegerType)count_I_LSB_DL[-1] = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 03 02 01 00

- No.: 2306
- Timestamp: 17:17:50:341_0
- RFN: 6904
- Chip: 33536
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 8
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 3
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 2307
- Timestamp: 17:17:50:341_1
- RFN: 6904
- Chip: 35584
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 9
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 4
. (IntegerType)count_I_LSB_UL[-1] = -
. (IntegerType)count_I_LSB_DL[-1] = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 04 02 01 00

- No.: 2308
- Timestamp: 17:17:50:342_0
- RFN: 6904
- Chip: 37632
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 10
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 4
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 2312
- Timestamp: 17:17:50:343_0
- RFN: 6905
- Chip: 2816
- Event: Send
- PCO: CRLC
- Message: CRLC_Integrity_Activate_REQ
- Source: ts_CRLC_DL_Integrity LINE 1
- Message Structure:
CRLC_Integrity_Activate_REQ
. (IntegerType)cellId[-1] = -1
. (CN_DomainIdentity)cn_DomainIdentity[0] = 1
. IntegrityActivationInfo
. . IntegrityProtectionModeInfo
. . . IntegrityProtectionModeCommand
. . . . startIntegrityProtection
. . . . . (BitStringType)integrityProtInitNumber[32] = "00000000000000000000000000000001"
. . . (IntegrityProtectionAlgorithm)integrityProtectionAlgorithm[0] = 0
- Constraint:
ca_CRLC_DL_IntegrityActivateReq
- BinaryMessage:
30 14 02 01 ff 0a 01 01 30 0c 30 07 03 05 00 00 00 00 01 0a 01 00

- No.: 2313
- Timestamp: 17:17:50:343_1
- RFN: 6905
- Chip: 4608
- Event: Receive
- PCO: CRLC
- Message: CRLC_Integrity_Activate_CNF
- Source: ts_CRLC_DL_Integrity LINE 2
- Message Structure:
CRLC_Integrity_Activate_CNF
. (IntegerType)cellId[0] = -1
- Constraint:
ca_CRLC_IntegrityActivateCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 2320
- Timestamp: 17:17:50:345_0
- RFN: 6905
- Chip: 9728
- Event: Send
- PCO: CRLC
- Message: CRLC_Integrity_Activate_REQ
- Source: ts_RB2_UL_IntegrityActivate LINE 1
- Message Structure:
CRLC_Integrity_Activate_REQ
. (IntegerType)cellId[-1] = -1
. (CN_DomainIdentity)cn_DomainIdentity[0] = 1
. IntegrityActivationInfo
. . IntegrityProtActivationInfoList
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity[-1] = 2
. . . . (IntegerType)rrc_MessageSequenceNumber[-1] = 0
- Constraint:
ca_CRLC_UL_IntegrityActivateReq
- BinaryMessage:
30 10 02 01 ff 0a 01 01 30 08 30 06 02 01 02 02 01 00

- No.: 2321
- Timestamp: 17:17:50:345_1
- RFN: 6905
- Chip: 11264
- Event: Receive
- PCO: CRLC
- Message: CRLC_Integrity_Activate_CNF
- Source: ts_RB2_UL_IntegrityActivate LINE 2
- Message Structure:
CRLC_Integrity_Activate_CNF
. (IntegerType)cellId[0] = -1
- Constraint:
ca_CRLC_IntegrityActivateCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 2328
- Timestamp: 17:17:50:347_0
- RFN: 6905
- Chip: 18176
- Event: Send
- PCO: AM
- Message: RLC_AM_DATA_REQ
- Source: ts_RRC_Security:lt_SendSecurityModeCommand LINE 16
- Message Structure:
RLC_AM_DATA_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 2
. AmConfirmationRequest
. aM_message
. . DL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00000000000000000000000000000000"
. . . . (IntegerType)rrc_MessageSequenceNumber[-1] = 0
. . . DL_DCCH_MessageType
. . . . SecurityModeCommand
. . . . . r3
. . . . . . SecurityModeCommand_r3_IEs
. . . . . . . (IntegerType)rrc_TransactionIdentifier[-1] = 0
. . . . . . . SecurityCapability
. . . . . . . . (BitStringType)cipheringAlgorithmCap[16] = '0000000000000011'B
. . . . . . . . (BitStringType)integrityProtectionAlgorithmCap[16] = '0000000000000010'B
. . . . . . . CipheringModeInfo
. . . . . . . IntegrityProtectionModeInfo
. . . . . . . . IntegrityProtectionModeCommand
. . . . . . . . . startIntegrityProtection
. . . . . . . . . . (BitStringType)integrityProtInitNumber[32] = "00000000000000000000000000000001"
. . . . . . . . (IntegrityProtectionAlgorithm)integrityProtectionAlgorithm[0] = 0
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity[0] = 1
. . . . . . . InterRAT_UE_SecurityCapList
. . . . . . laterNonCriticalExtensions
- Constraint:
cas_RRC_SecModeCmd
- BinaryMessage:
30 17 02 01 ff 02 01 02 05 00 80 00 00 00 04 04 00 01 80 01 40 00 00 00 30

- No.: 2337
- Timestamp: 17:17:50:470_0
- RFN: 6917
- Chip: 31488
- Event: Receive
- PCO: AM
- Message: RLC_AM_DATA_IND
- Source: ts_RRC_Security:lt_StartSecurity_UE LINE 8
- Message Structure:
RLC_AM_DATA_IND
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 2
. IntegrityResult
. . (IntegrityStatus)integrityUsed[0] = 0
. aM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "10000001100000001110110111011101"
. . . . (IntegerType)rrc_MessageSequenceNumber[4] = 1
. . . UL_DCCH_MessageType
. . . . SecurityModeComplete
. . . . . (IntegerType)rrc_TransactionIdentifier[2] = 0
. . . . . IntegrityProtActivationInfo
. . . . . . RRC_MessageSequenceNumberList
. . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . (IntegerType)_elem[4] = 0
. . . . . laterNonCriticalExtensions
- Constraint:
car_RRC_SecModeCmpl
- BinaryMessage:
30 12 02 01 ff 02 01 02 0a 01 00 c0 c0 76 ee 8d 21 00 00 00

- No.: 2338
- Timestamp: 17:17:50:470_1
- RFN: 6917
- Chip: 33024
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_Security:lt_StartSecurity_UE LINE 8
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2340
- Timestamp: 17:17:50:471_1
- RFN: 6917
- Chip: 36608
- Event: Send
- PCO: CRLC
- Message: CRLC_Integrity_Activate_REQ
- Source: ts_CRLC_UL_Integrity LINE 1
- Message Structure:
CRLC_Integrity_Activate_REQ
. (IntegerType)cellId[-1] = -1
. (CN_DomainIdentity)cn_DomainIdentity[0] = 1
. IntegrityActivationInfo
. . IntegrityProtActivationInfoList
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity[-1] = 0
. . . . (IntegerType)rrc_MessageSequenceNumber[-1] = 0
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity[-1] = 1
. . . . (IntegerType)rrc_MessageSequenceNumber[-1] = 0
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity[-1] = 3
. . . . (IntegerType)rrc_MessageSequenceNumber[-1] = 0
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity[-1] = 4
. . . . (IntegerType)rrc_MessageSequenceNumber[-1] = 0
- Constraint:
ca_CRLC_UL_IntegrityActivateReq
- BinaryMessage:
30 28 02 01 ff 0a 01 01 30 20 30 06 02 01 00 02 01 00 30 06 02 01 01 02 01 00 30 06 02 01 03 02 01 00 30 06 02 01 04 02 01 00

- No.: 2341
- Timestamp: 17:17:50:472_0
- RFN: 6918
- Chip: 256
- Event: Receive
- PCO: CRLC
- Message: CRLC_Integrity_Activate_CNF
- Source: ts_CRLC_UL_Integrity LINE 2
- Message Structure:
CRLC_Integrity_Activate_CNF
. (IntegerType)cellId[0] = -1
- Constraint:
ca_CRLC_IntegrityActivateCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 2347
- Timestamp: 17:17:50:473_0
- RFN: 6918
- Chip: 6400
- Event: Send
- PCO: Dc
- Message: RRC_DataReq
- Source: tc_12_4_1_4c2:lt_Attach_Steps_3To4 LINE 4
- Message Structure:
RRC_DataReq
. (IntegerType)cellId[-1] = -1
. (SS_RB_Identity)rB_Id[-1] = 3
. (LogicChGERAN)ch[-1] = -
. (SapId)sapId[1] = -
. (SS_CN_DomainIdentity)cN_Domain[-1] = 1
. ATTACHACCEPT
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)gMMProtocolDiscriminator[4] = '1000'B
. . (MsgType)msgType[8] = '00000010'B
. . ForceToStandby
. . . (B1)spare[1] = '0'B
. . . (B3)value[3] = '000'B
. . AttachResult
. . . (B1)spare[1] = '0'B
. . . (B3)result[3] = '011'B
. . GPRS_Timer_v
. . . (B3)unit[3] = '001'B
. . . (B5)value[5] = '00110'B
. . (B4)spare[4] = '0000'B
. . RadioPriority_v
. . . (B1)spare[1] = '0'B
. . . (B3)value[3] = '100'B
. . RAI_v
. . . (OctetStringType)plmn[3] = '00F110'O
. . . (OctetStringType)lac[2] = '0001'O
. . . (OctetStringType)rac[1] = '05'O
. . PTMSI_Signature
. . . (IEI8)iei[8] = '00011001'B
. . . (OctetStringType)value[3] = 'AB1237'O
. . GPRS_Timer
. . GMM_MS_IdentityPTMSI
. . . (IEI8)iei[8] = '00011000'B
. . . (Length)iel[1] = '05'O
. . . (B4)iDigit1[4] = '1111'B
. . . (B1)oddEvenInd[1] = '0'B
. . . (B3)typeOfId[3] = '100'B
. . . (OctetStringType)otherDigits[-1] = '09876543'O
. . GMM_MS_Identity
. . . (IEI8)iei[8] = '00100011'B
. . . (Length)iel[1] = '08'O
. . . (B4)iDigit1[4] = '0000'B
. . . (B1)oddEvenInd[1] = '1'B
. . . (B3)typeOfId[3] = '001'B
. . . (OctetStringType)otherDigits[-1] = '10101032540636'O
. . GMM_Cause
. . GPRS_Timer
. . CellNotification
. . PLMN_List
- Constraint:
ca_PS_DataReq
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 08 02 03 26 04 00 f1 10 00 01 05 19 ab 12 37 18 05 f4 09 87 65 43 23 08 09 10 10 10 32 54 06 36

- No.: 2354
- Timestamp: 17:17:50:620_0
- RFN: 6932
- Chip: 28672
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: tc_12_4_1_4c2:lt_Attach_Steps_3To4 LINE 5
- Message Structure:
RRC_DataInd
. (IntegerType)cellId[0] = -1
. (SS_RB_Identity)rB_Id[0] = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain[0] = 1
. (START_Value)start[0] = -
. ATTACHCOMPLETE
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)gMMProtocolDiscriminator[4] = '1000'B
. . (MsgType)msgType[8] = '00000011'B
- Constraint:
car_PS_UplinkDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 08 03

- No.: 2362
- Timestamp: 17:17:50:621_2
- RFN: 6932
- Chip: 33024
- Event: Start Timer
- Source: ts_RRC_Delay LINE 1
- Message Structure:
no details available
- Constraint:
t_Dly (1000 Ms)
- BinaryMessage:

- No.: 2366
- Timestamp: 17:17:51:622_0
- RFN: 7032
- Chip: 37888
- Event: Timeout
- Source: ts_RRC_Delay LINE 2
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 2371
- Timestamp: 17:17:51:623_0
- RFN: 7033
- Chip: 4864
- Event: Send
- PCO: UM
- Message: RLC_UM_DATA_REQ
- Source: ts_RRC_ConnRel:lt_Send_RRC_ConnectionRelease LINE 3
- Message Structure:
RLC_UM_DATA_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 1
. uM_message
. . DL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00000000000000000000000000000000"
. . . . (IntegerType)rrc_MessageSequenceNumber[-1] = 0
. . . DL_DCCH_MessageType
. . . . RRCConnectionRelease
. . . . . r3
. . . . . . RRCConnectionRelease_r3_IEs
. . . . . . . (IntegerType)rrc_TransactionIdentifier[-1] = 0
. . . . . . . (IntegerType)n_308[-1] = 1
. . . . . . . (ReleaseCause)releaseCause[0] = 0
. . . . . . . Rplmn_Information
. . . . . . laterNonCriticalExtensions
. (BooleanType)specialLI = FALSE
- Constraint:
cas_RRC_ConnRelDCCH
- BinaryMessage:
30 10 02 01 ff 02 01 01 80 00 00 00 03 c8 00 01 01 00

- No.: 2375
- Timestamp: 17:17:51:751_0
- RFN: 7045
- Chip: 30720
- Event: Receive
- PCO: UM
- Message: RLC_UM_DATA_IND
- Source: ts_RRC_ConnRel:lt_Send_RRC_ConnectionRelease LINE 4
- Message Structure:
RLC_UM_DATA_IND
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 1
. IntegrityResult
. uM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "10101101101011101001000000111001"
. . . . (IntegerType)rrc_MessageSequenceNumber[4] = 1
. . . UL_DCCH_MessageType
. . . . RRCConnectionReleaseComplete
. . . . . (IntegerType)rrc_TransactionIdentifier[2] = 0
. . . . . FailureCauseWithProtErr
. . . . . laterNonCriticalExtensions
- Constraint:
car_RRC_ConnRelCmplUM
- BinaryMessage:
30 0e 02 01 ff 02 01 01 05 00 d6 d7 48 1c 8c 40

- No.: 2376
- Timestamp: 17:17:51:751_1
- RFN: 7045
- Chip: 32000
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ConnRel:lt_Send_RRC_ConnectionRelease LINE 4
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2379
- Timestamp: 17:17:51:751_4
- RFN: 7045
- Chip: 34048
- Event: Start Timer
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 1
- Message Structure:
no details available
- Constraint:
t_Dly (5000 Ms)
- BinaryMessage:

- No.: 2383
- Timestamp: 17:17:51:910_0
- RFN: 7061
- Chip: 30720
- Event: Receive
- PCO: UM
- Message: RLC_UM_DATA_IND
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 4
- Message Structure:
RLC_UM_DATA_IND
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 1
. IntegrityResult
. uM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00011100010101000111110101101001"
. . . . (IntegerType)rrc_MessageSequenceNumber[4] = 2
. . . UL_DCCH_MessageType
. . . . RRCConnectionReleaseComplete
. . . . . (IntegerType)rrc_TransactionIdentifier[2] = 0
. . . . . FailureCauseWithProtErr
. . . . . laterNonCriticalExtensions
- Constraint:
car_RRC_ConnRelCmplUM
- BinaryMessage:
30 0e 02 01 ff 02 01 01 05 00 8e 2a 3e b4 94 40

- No.: 2384
- Timestamp: 17:17:51:910_1
- RFN: 7061
- Chip: 32000
- Event: Cancel Timer
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 4
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 2385
- Timestamp: 17:17:51:910_2
- RFN: 7061
- Chip: 32512
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 4
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2391
- Timestamp: 17:17:51:912_0
- RFN: 7061
- Chip: 36864
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 1
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 01 0a 01 00 05 00

- No.: 2395
- Timestamp: 17:17:51:918_0
- RFN: 7062
- Chip: 21760
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 2398
- Timestamp: 17:17:51:919_0
- RFN: 7062
- Chip: 25088
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 2
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 02 0a 01 00 05 00

- No.: 2402
- Timestamp: 17:17:51:923_0
- RFN: 7063
- Chip: 2560
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 2405
- Timestamp: 17:17:51:923_3
- RFN: 7063
- Chip: 5888
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 3
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 03 0a 01 00 05 00

- No.: 2409
- Timestamp: 17:17:51:929_0
- RFN: 7063
- Chip: 25856
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 3
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 2412
- Timestamp: 17:17:51:930_0
- RFN: 7063
- Chip: 29440
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 4
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 04 0a 01 00 05 00

- No.: 2416
- Timestamp: 17:17:51:936_0
- RFN: 7064
- Chip: 14080
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 4
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 2419
- Timestamp: 17:17:51:937_0
- RFN: 7064
- Chip: 19968
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 1
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 136
. . . . . UL_RLC_Mode
. . . . . . UL_UM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (NoExplicitDiscard)timerBasedNoExplicit[0] = 9
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 1
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 1
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_UM_Info
- BinaryMessage:
30 22 02 01 ff 02 01 01 0a 01 00 30 17 30 0d 05 00 30 09 02 02 00 88 30 03 0a 01 09 30 06 02 01 01 02 01 01

- No.: 2423
- Timestamp: 17:17:51:942_0
- RFN: 7065
- Chip: 768
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 2424
- Timestamp: 17:17:51:944_0
- RFN: 7065
- Chip: 7680
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 3
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 2
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 2
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 2
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 02 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 13 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 02 02 01 02

- No.: 2428
- Timestamp: 17:17:51:952_0
- RFN: 7065
- Chip: 37888
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 4
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 2429
- Timestamp: 17:17:51:953_0
- RFN: 7066
- Chip: 5888
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 5
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 3
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 3
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 3
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 03 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 13 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 03 02 01 03

- No.: 2433
- Timestamp: 17:17:51:962_0
- RFN: 7066
- Chip: 37632
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 6
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 3
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 2434
- Timestamp: 17:17:51:963_0
- RFN: 7067
- Chip: 6144
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 7
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 4
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 4
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 4
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 04 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 13 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 04 02 01 04

- No.: 2438
- Timestamp: 17:17:51:972_0
- RFN: 7068
- Chip: 1536
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 8
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 4
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 2462
- Timestamp: 17:17:51:975_5
- RFN: 7068
- Chip: 13056
- Event: Start Timer
- Source: tc_12_4_1_4c2:lt_TestBody LINE 5
- Message Structure:
no details available
- Constraint:
t_UpperBound (396000 Ms)
- BinaryMessage:

- No.: 2463
- Timestamp: 17:17:51:975_6
- RFN: 7068
- Chip: 13568
- Event: Start Timer
- Source: tc_12_4_1_4c2:lt_TestBody LINE 5
- Message Structure:
no details available
- Constraint:
t_LowerBound (324000 Ms)
- BinaryMessage:

- No.: 2475
- Timestamp: 17:23:15:964_1
- RFN: 39470
- Chip: 512
- Event: Timeout
- Source: tc_12_4_1_4c2:lt_RARej LINE 1
- Message Structure:
no details available
- Constraint:
t_LowerBound
- BinaryMessage:

- No.: 2479
- Timestamp: 17:23:53:328_0
- RFN: 43206
- Chip: 28416
- Event: Receive
- PCO: TM
- Message: RLC_TR_DATA_IND
- Source: tc_12_4_1_4c2:lt_RARej LINE 2
- Message Structure:
RLC_TR_DATA_IND
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 0
. tM_message
. . UL_CCCH_Message
. . . IntegrityCheckInfo
. . . UL_CCCH_MessageType
. . . . RRCConnectionRequest
. . . . . InitialUE_Identity
. . . . . . P_TMSI_and_RAI_GSM_MAP
. . . . . . . (BitStringType)p_TMSI[32] = "00001001100001110110010101000011"
. . . . . . . RAI
. . . . . . . . LAI
. . . . . . . . . PLMN_Identity
. . . . . . . . . . MCC
. . . . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . . . (IntegerType)_elem[4] = 1
. . . . . . . . . . MNC
. . . . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . . . (IntegerType)_elem[4] = 1
. . . . . . . . . (BitStringType)lac[16] = '0000000000000001'B
. . . . . . . . (BitStringType)rac[8] = "00000101"
. . . . . (EstablishmentCause)establishmentCause[5] = 12
. . . . . (ProtocolErrorIndicator)protocolErrorIndicator[1] = 0
. . . . . MeasuredResultsOnRACH
. . . . . v3d0NonCriticalExtensions
- Constraint:
car_RRC_ConnReq
- BinaryMessage:
30 12 02 01 00 02 01 00 22 09 87 65 43 00 10 08 00 08 2b 00

- No.: 2480
- Timestamp: 17:23:53:328_1
- RFN: 43206
- Chip: 30464
- Event: Cancel Timer
- Source: tc_12_4_1_4c2:lt_RARej LINE 2
- Message Structure:
no details available
- Constraint:
t_UpperBound
- BinaryMessage:

- No.: 2481
- Timestamp: 17:23:53:328_2
- RFN: 43206
- Chip: 30976
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: tc_12_4_1_4c2:lt_RARej LINE 2
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2496
- Timestamp: 17:23:53:341_0
- RFN: 43208
- Chip: 2304
- Event: Send
- PCO: UM
- Message: RLC_UM_DATA_REQ
- Source: ts_RRC_ConnEstEnd:lt_Send_ConnSetUp LINE 22
- Message Structure:
RLC_UM_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 0
. uM_message
. . DL_CCCH_Message
. . . IntegrityCheckInfo
. . . DL_CCCH_MessageType
. . . . RRCConnectionSetup
. . . . . r3
. . . . . . RRCConnectionSetup_r3_IEs
. . . . . . . InitialUE_Identity
. . . . . . . . P_TMSI_and_RAI_GSM_MAP
. . . . . . . . . (BitStringType)p_TMSI[32] = "00001001100001110110010101000011"
. . . . . . . . . RAI
. . . . . . . . . . LAI
. . . . . . . . . . . PLMN_Identity
. . . . . . . . . . . . MCC
. . . . . . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . . . . . (IntegerType)_elem[4] = 1
. . . . . . . . . . . . MNC
. . . . . . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . . . . . (IntegerType)_elem[4] = 1
. . . . . . . . . . . (BitStringType)lac[16] = '0000000000000001'B
. . . . . . . . . . (BitStringType)rac[8] = "00000101"
. . . . . . . (IntegerType)rrc_TransactionIdentifier[-1] = 0
. . . . . . . (IntegerType)activationTime[-1] = -
. . . . . . . U_RNTI
. . . . . . . . (BitStringType)srnc_Identity[12] = "000000000001"
. . . . . . . . (BitStringType)s_RNTI[20] = "00000000000000000001"
. . . . . . . (BitStringType)new_c_RNTI[16] = -
. . . . . . . (RRC_StateIndicator)rrc_StateIndicator[0] = 0
. . . . . . . (IntegerType)utran_DRX_CycleLengthCoeff[-1] = 9
. . . . . . . CapabilityUpdateRequirement
. . . . . . . . (BooleanType)ue_RadioCapabilityFDDUpdateRequirement = TRUE
. . . . . . . . (BooleanType)ue_RadioCapabilityTDDUpdateRequirement = FALSE
. . . . . . . . SystemSpecificCapUpdateReqList
. . . . . . . . . (SystemSpecificCapUpdateReq)_elem[0] = 0
. . . . . . . SRB_InformationSetupList2
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity[-1] = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_UM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 1
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex[-1] = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 1
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity[-1] = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 2
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 2
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 2
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 2
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex[-1] = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 2
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 2
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity[-1] = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 3
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 3
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 3
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 3
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex[-1] = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 3
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 3
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity[-1] = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 4
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 4
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 4
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 4
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex[-1] = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 4
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 4
. . . . . . . UL_CommonTransChInfo
. . . . . . . . TFC_Subset
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . TFCS
. . . . . . . . . . . ExplicitTFCS_Configuration
. . . . . . . . . . . . TFCS_ReconfAdd
. . . . . . . . . . . . . ctfcSize
. . . . . . . . . . . . . . ctfc2Bit
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . . . . . . . (IntegerType)ctfc2[-1] = 0
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . . . . . . . (IntegerType)ctfc2[-1] = 1
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC[-1] = 11
. . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaD[-1] = 15
. . . . . . . . . . . . . . . . . . . (IntegerType)referenceTFC_ID[-1] = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . UL_AddReconfTransChInfoList
. . . . . . . . UL_AddReconfTransChInformation
. . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType[0] = 0
. . . . . . . . . (IntegerType)transportChannelIdentity[-1] = 5
. . . . . . . . . TransportFormatSet
. . . . . . . . . . DedicatedTransChTFS
. . . . . . . . . . . tti
. . . . . . . . . . . . DedicatedDynamicTF_InfoList
. . . . . . . . . . . . . DedicatedDynamicTF_Info
. . . . . . . . . . . . . . rlc_Size
. . . . . . . . . . . . . . . BitModeRLC_SizeInfo
. . . . . . . . . . . . . . . . sizeType2
. . . . . . . . . . . . . . . . . (IntegerType)part1[-1] = 2
. . . . . . . . . . . . . . . . . (IntegerType)part2[-1] = -
. . . . . . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . LogicalChannelList
. . . . . . . . . . . SemistaticTF_Information
. . . . . . . . . . . . ChannelCodingType
. . . . . . . . . . . . . (CodingRate)convolutional[0] = 1
. . . . . . . . . . . . (IntegerType)rateMatchingAttribute[-1] = 192
. . . . . . . . . . . . (CRC_Size)crc_Size[0] = 3
. . . . . . . DL_CommonTransChInfo
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . dl_Parameters
. . . . . . . DL_AddReconfTransChInfoList
. . . . . . . . DL_AddReconfTransChInformation
. . . . . . . . . (DL_TrCH_Type)dl_TransportChannelType[0] = 0
. . . . . . . . . (IntegerType)dl_transportChannelIdentity[-1] = 10
. . . . . . . . . tfs_SignallingMode
. . . . . . . . . . UL_TransportChannelIdentity
. . . . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType[0] = 0
. . . . . . . . . . . (IntegerType)ul_TransportChannelIdentity[-1] = 5
. . . . . . . . . QualityTarget
. . . . . . . . . . (IntegerType)bler_QualityValue[-1] = -20
. . . . . . . . . TM_SignallingInfo
. . . . . . . FrequencyInfo
. . . . . . . (IntegerType)maxAllowedUL_TX_Power[-1] = -
. . . . . . . UL_ChannelRequirement
. . . . . . . . UL_DPCH_Info
. . . . . . . . . UL_DPCH_PowerControlInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (IntegerType)dpcch_PowerOffset[-1] = -40
. . . . . . . . . . . (IntegerType)pc_Preamble[-1] = 1
. . . . . . . . . . . (IntegerType)sRB_delay[-1] = 7
. . . . . . . . . . . PowerControlAlgorithm
. . . . . . . . . . . . (IntegerType)algorithm1[-1] = 1
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (ScramblingCodeType)scramblingCodeType[0] = 1
. . . . . . . . . . . (IntegerType)scramblingCode[-1] = 0
. . . . . . . . . . . (IntegerType)numberOfDPDCH[-1] = -
. . . . . . . . . . . (SpreadingFactor)spreadingFactor[0] = 4
. . . . . . . . . . . (BooleanType)tfci_Existence = TRUE
. . . . . . . . . . . (IntegerType)numberOfFBI_Bits[-1] = -
. . . . . . . . . . . (PuncturingLimit)puncturingLimit[0] = 15
. . . . . . . DL_CommonInformation
. . . . . . . . DL_DPCH_InfoCommon
. . . . . . . . . cfnHandling
. . . . . . . . . . initialise
. . . . . . . . . . . (IntegerType)cfntargetsfnframeoffset[-1] = -
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . DL_DPCH_PowerControlInfo
. . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . (DPC_Mode)dpc_Mode[0] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPilot_pdpdch[-1] = 0
. . . . . . . . . . . Dl_rate_matching_restriction
. . . . . . . . . . . SF512_AndPilot
. . . . . . . . . . . . (PilotBits128)sfd128[0] = 0
. . . . . . . . . . . (PositionFixedOrFlexible)positionFixedOrFlexible[0] = 0
. . . . . . . . . . . (BooleanType)tfci_Existence = FALSE
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . (IntegerType)defaultDPCH_OffsetValue[-1] = 459
. . . . . . . . . . DPCH_CompressedModeInfo
. . . . . . . . . . (TX_DiversityMode)tx_DiversityMode[0] = 0
. . . . . . . . . . SSDT_Information
. . . . . . . DL_InformationPerRL_List
. . . . . . . . DL_InformationPerRL
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . PrimaryCPICH_Info
. . . . . . . . . . . . (IntegerType)primaryScramblingCode[-1] = 100
. . . . . . . . . . . PDSCH_SHO_DCH_Info
. . . . . . . . . . . PDSCH_CodeMapping
. . . . . . . . . DL_DPCH_InfoPerRL
. . . . . . . . . . fdd
. . . . . . . . . . . (PCPICH_UsageForChannelEst)pCPICH_UsageForChannelEst[0] = 0
. . . . . . . . . . . (IntegerType)dpch_FrameOffset[-1] = 18
. . . . . . . . . . . SecondaryCPICH_Info
. . . . . . . . . . . DL_ChannelisationCodeList
. . . . . . . . . . . . DL_ChannelisationCode
. . . . . . . . . . . . . (IntegerType)secondaryScramblingCode[-1] = 1
. . . . . . . . . . . . . SF512_AndCodeNumber
. . . . . . . . . . . . . . (IntegerType)sf128[-1] = 0
. . . . . . . . . . . . . (ScramblingCodeChange)scramblingCodeChange[0] = 1
. . . . . . . . . . . (IntegerType)tpc_CombinationIndex[-1] = 0
. . . . . . . . . . . (SSDT_CellIdentity)ssdt_CellIdentity[0] = -
. . . . . . . . . . . (ClosedLoopTimingAdjMode)closedLoopTimingAdjMode[0] = -
. . . . . . . . . SCCPCH_InfoForFACH
. . . . . . laterNonCriticalExtensions
. (BooleanType)specialLI = TRUE
- Constraint:
cas_RRC_ConnSetup
- BinaryMessage:
30 79 02 01 00 02 01 00 30 e7 41 30 ec a8 60 02 01 00 01 05 00 04 00 00 4d 82 69 3a 10 10 89 0d 42 00 02 81 9e 8e 46 c9 a6 7c 9c 4e 74 20 a5 12 3a 8c 00 15 13 3d 1c 8d 93 4c f9 38 9c e8 42 52 24 b5 28 00 4a 46 7a 39 1b 26 99 f2 71 39 d0 86 b4 49 ea 70 00 d4 c8 00 06 25 2b f0 02 00 08 82 23 bf 66 08 98 95 a5 47 a2 00 00 01 3f 90 0a 14 e5 82 06 40 09 0c 28 08 01 01 ff

- No.: 2517
- Timestamp: 17:23:53:364_0
- RFN: 43210
- Chip: 12800
- Event: Start Timer
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 3
- Message Structure:
no details available
- Constraint:
t_WaitMS (13500 Ms)
- BinaryMessage:

- No.: 2519
- Timestamp: 17:23:53:364_2
- RFN: 43210
- Chip: 14848
- Event: Receive
- PCO: CPHY
- Message: CPHY_Out_of_Sync_IND
- Source: RRC_DefConnEst LINE 7
- Message Structure:
CPHY_Out_of_Sync_IND
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 20
- Constraint:
ca_OutOfSyncInd
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 2520
- Timestamp: 17:23:53:364_3
- RFN: 43210
- Chip: 15616
- Event: Cancel Timer
- Source: RRC_DefConnEst LINE 7
- Message Structure:
no details available
- Constraint:
t_T312
- BinaryMessage:

- No.: 2521
- Timestamp: 17:23:53:364_4
- RFN: 43210
- Chip: 16384
- Event: Default
- Source: RRC_DefConnEst LINE 0
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2522
- Timestamp: 17:23:53:365_0
- RFN: 43210
- Chip: 16640
- Event: Default
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2530
- Timestamp: 17:23:53:568_1
- RFN: 43230
- Chip: 27904
- Event: Receive
- PCO: CPHY
- Message: CPHY_Sync_IND
- Source: RRC_DefConnEst LINE 5
- Message Structure:
CPHY_Sync_IND
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 20
- Constraint:
ca_SyncInd
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 2531
- Timestamp: 17:23:53:568_2
- RFN: 43230
- Chip: 28672
- Event: Cancel Timer
- Source: RRC_DefConnEst LINE 5
- Message Structure:
no details available
- Constraint:
t_T312
- BinaryMessage:

- No.: 2532
- Timestamp: 17:23:53:568_3
- RFN: 43230
- Chip: 29440
- Event: Default
- Source: RRC_DefConnEst LINE 0
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2533
- Timestamp: 17:23:53:568_4
- RFN: 43230
- Chip: 29696
- Event: Default
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2540
- Timestamp: 17:23:53:669_0
- RFN: 43240
- Chip: 34816
- Event: Receive
- PCO: AM
- Message: RLC_AM_DATA_IND
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
RLC_AM_DATA_IND
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 2
. IntegrityResult
. . (IntegrityStatus)integrityUsed[0] = 4294967296
. aM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . UL_DCCH_MessageType
. . . . RRCConnectionSetupComplete
. . . . . (IntegerType)rrc_TransactionIdentifier[2] = 0
. . . . . STARTList
. . . . . . STARTSingle
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity[1] = 1
. . . . . . . (BitStringType)start_Value[20] = "00000000000000000010"
. . . . . . STARTSingle
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity[1] = 0
. . . . . . . (BitStringType)start_Value[20] = "00000000000000000010"
. . . . . UE_RadioAccessCapability
. . . . . . (AccessStratumReleaseIndicator)accessStratumReleaseIndicator[0] = 0
. . . . . . PDCP_Capability
. . . . . . . (BooleanType)losslessSRNS_RelocationSupport = FALSE
. . . . . . . supportForRfc2507
. . . . . . . . (MaxHcContextSpace)supported[3] = 4
. . . . . . RLC_Capability
. . . . . . . (TotalRLC_AM_BufferSize)totalRLC_AM_BufferSize[3] = 2
. . . . . . . (MaximumRLC_WindowSize)maximumRLC_WindowSize[1] = 0
. . . . . . . (MaximumAM_EntityNumberRLC_Cap)maximumAM_EntityNumber[3] = 3
. . . . . . TransportChannelCapability
. . . . . . . DL_TransChCapability
. . . . . . . . (MaxNoBits)maxNoBitsReceived[4] = 7
. . . . . . . . (MaxNoBits)maxConvCodeBitsReceived[4] = 1
. . . . . . . . TurboSupport
. . . . . . . . . (MaxNoBits)supported[4] = 7
. . . . . . . . (MaxSimultaneousTransChsDL)maxSimultaneousTransChs[2] = 1
. . . . . . . . (IntegerType)maxSimultaneousCCTrCH_Count[3] = 1
. . . . . . . . (MaxTransportBlocksDL)maxReceivedTransportBlocks[4] = 3
. . . . . . . . (MaxNumberOfTFC_DL)maxNumberOfTFC[4] = 5
. . . . . . . . (MaxNumberOfTF)maxNumberOfTF[3] = 1
. . . . . . . UL_TransChCapability
. . . . . . . . (MaxNoBits)maxNoBitsTransmitted[4] = 3
. . . . . . . . (MaxNoBits)maxConvCodeBitsTransmitted[4] = 1
. . . . . . . . TurboSupport
. . . . . . . . . (MaxNoBits)supported[4] = 3
. . . . . . . . (MaxSimultaneousTransChsUL)maxSimultaneousTransChs[3] = 2
. . . . . . . . modeSpecificInfo
. . . . . . . . (MaxTransportBlocksUL)maxTransmittedBlocks[4] = 4
. . . . . . . . (MaxNumberOfTFC_UL)maxNumberOfTFC[4] = 5
. . . . . . . . (MaxNumberOfTF)maxNumberOfTF[3] = 0
. . . . . . RF_Capability
. . . . . . . fddRF_Capability
. . . . . . . . (IntegerType)ue_PowerClass[2] = 4
. . . . . . . . (TxRxFrequencySeparation)txRxFrequencySeparation[2] = 0
. . . . . . . tddRF_Capability
. . . . . . PhysicalChannelCapability
. . . . . . . fddPhysChCapability
. . . . . . . . DL_PhysChCapabilityFDD
. . . . . . . . . (IntegerType)maxNoDPCH_PDSCH_Codes[3] = 1
. . . . . . . . . (MaxNoPhysChBitsReceived)maxNoPhysChBitsReceived[4] = 6
. . . . . . . . . (BooleanType)supportForSF_512 = FALSE
. . . . . . . . . (BooleanType)supportOfPDSCH = FALSE
. . . . . . . . . SimultaneousSCCPCH_DPCH_Reception
. . . . . . . . UL_PhysChCapabilityFDD
. . . . . . . . . (MaxNoDPDCH_BitsTransmitted)maxNoDPDCH_BitsTransmitted[4] = 3
. . . . . . . . . (BooleanType)supportOfPCPCH = FALSE
. . . . . . . tddPhysChCapability
. . . . . . UE_MultiModeRAT_Capability
. . . . . . . MultiRAT_Capability
. . . . . . . . (BooleanType)supportOfGSM = FALSE
. . . . . . . . (BooleanType)supportOfMulticarrier = FALSE
. . . . . . . (MultiModeCapability)multiModeCapability[2] = 1
. . . . . . SecurityCapability
. . . . . . . (BitStringType)cipheringAlgorithmCap[16] = '0000000000000011'B
. . . . . . . (BitStringType)integrityProtectionAlgorithmCap[16] = '0000000000000010'B
. . . . . . UE_Positioning_Capability
. . . . . . . (BooleanType)standaloneLocMethodsSupported = FALSE
. . . . . . . (BooleanType)ue_BasedOTDOA_Supported = FALSE
. . . . . . . (NetworkAssistedGPS_Supported)networkAssistedGPS_Supported[2] = 3
. . . . . . . (BooleanType)supportForUE_GPS_TimingOfCellFrames = FALSE
. . . . . . . (BooleanType)supportForIPDL = FALSE
. . . . . . MeasurementCapability
. . . . . . . CompressedModeMeasCapability
. . . . . . . . (BooleanType)fdd_Measurements = TRUE
. . . . . . . . (BooleanType)tdd_Measurements = -
. . . . . . . . GSM_Measurements
. . . . . . . . . (BooleanType)gsm900 = TRUE
. . . . . . . . . (BooleanType)dcs1800 = TRUE
. . . . . . . . . (BooleanType)gsm1900 = TRUE
. . . . . . . . (BooleanType)multiCarrierMeasurements = FALSE
. . . . . . . CompressedModeMeasCapability
. . . . . . . . (BooleanType)fdd_Measurements = TRUE
. . . . . . . . (BooleanType)tdd_Measurements = -
. . . . . . . . GSM_Measurements
. . . . . . . . . (BooleanType)gsm900 = TRUE
. . . . . . . . . (BooleanType)dcs1800 = TRUE
. . . . . . . . . (BooleanType)gsm1900 = TRUE
. . . . . . . . (BooleanType)multiCarrierMeasurements = FALSE
. . . . . v370NonCriticalExtensions
- Constraint:
car_RRC_ConnSetupCmpl
- BinaryMessage:
30 27 02 01 ff 02 01 02 0a 05 01 00 00 00 00 4a 0c 00 00 80 00 05 62 37 1b a0 d4 98 cd 11 45 90 60 61 00 03 00 02 31 f9 f8

- No.: 2541
- Timestamp: 17:23:53:671_0
- RFN: 43241
- Chip: 3328
- Event: Cancel Timer
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
t_WaitMS
- BinaryMessage:

- No.: 2542
- Timestamp: 17:23:53:671_1
- RFN: 43241
- Chip: 3840
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2560
- Timestamp: 17:23:53:708_0
- RFN: 43244
- Chip: 32000
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: tc_12_4_1_4c2:lt_RARej LINE 4
- Message Structure:
RRC_DataInd
. (IntegerType)cellId[0] = -1
. (SS_RB_Identity)rB_Id[0] = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain[0] = 1
. (START_Value)start[20] = '00000000000000000010'B
. ROUTINGAREAUPDATEREQUEST
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)gMMProtocolDiscriminator[4] = '1000'B
. . (MsgType)msgType[8] = '00001000'B
. . CiphKeySeqNum
. . . (B1)spare1[1] = '0'B
. . . (KeySeq)keySeq[3] = '001'B
. . UpdateType_v
. . . (B1)pre_for[1] = '0'B
. . . (B3)value[3] = '011'B
. . RAI_v
. . . (OctetStringType)plmn[3] = '00F110'O
. . . (OctetStringType)lac[2] = '0001'O
. . . (OctetStringType)rac[1] = '05'O
. . MSRadioAccessCap_lv
. . . (Length)iel[1] = '0B'O
. . . (OctetStringType)value[11] = '15F38233542A332644A198'O
. . PTMSI_Signature
. . . (IEI8)iei[8] = '00011001'B
. . . (OctetStringType)value[3] = 'AB1237'O
. . GPRS_Timer
. . . (IEI8)iei[8] = '00010111'B
. . . (B3)unit[3] = '000'B
. . . (B5)value[5] = '10110'B
. . DRXparamter_tv
. . . (IEI8)iei[8] = '00100111'B
. . . (B8)splitPGcycleCode[8] = '00000111'B
. . . (B4)cnDRXcoef[4] = '0000'B
. . . (B1)splitOnCCCH[1] = '0'B
. . . (B3)nonDRXtimer[3] = '100'B
. . TMSI_Status
. . GMM_MS_IdentityPTMSI
. . . (IEI8)iei[8] = '00011000'B
. . . (Length)iel[1] = '05'O
. . . (B4)iDigit1[4] = '1111'B
. . . (B1)oddEvenInd[1] = '0'B
. . . (B3)typeOfId[3] = '100'B
. . . (OctetStringType)otherDigits[4] = '09876543'O
. . MS_NetworkCap_tlv
. . . (IEI8)iei[8] = '00110001'B
. . . (Length)iel[1] = '02'O
. . . (OctetStringType)value[2] = 'E540'O
. . PDP_ContextStatus
. . . (IEI8)iei[8] = '00110010'B
. . . (Length)iel[1] = '02'O
. . . (BitStringType)nSAPI[16] = '0000000000000000'B
- Constraint:
car_PS_InitDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 03 04 04 00 00 20 08 08 13 00 f1 10 00 01 05 0b 15 f3 82 33 54 2a 33 26 44 a1 98 19 ab 12 37 17 16 27 07 04 18 05 f4 09 87 65 43 31 02 e5 40 32 02 00 00

- No.: 2565
- Timestamp: 17:23:53:710_2
- RFN: 43245
- Chip: 1024
- Event: Send
- PCO: Dc
- Message: RRC_DataReq
- Source: tc_12_4_1_4c2:lt_RARej LINE 6
- Message Structure:
RRC_DataReq
. (IntegerType)cellId[-1] = -1
. (SS_RB_Identity)rB_Id[-1] = 3
. (LogicChGERAN)ch[-1] = -
. (SapId)sapId[1] = -
. (SS_CN_DomainIdentity)cN_Domain[-1] = 1
. ROUTING_AREA_UPDATE_REJECT
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)gMMProtocolDiscriminator[4] = '1000'B
. . (MsgType)msgType[8] = '00001011'B
. . (RejCau)gmmCause[1] = '0E'O
. . (B4)spare[4] = '0000'B
. . ForceToStandby
. . . (B1)spare[1] = '0'B
. . . (B3)value[3] = '000'B
. . GPRS_Timer
- Constraint:
ca_PS_DataReq
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 08 0b 0e 00

- No.: 2574
- Timestamp: 17:23:53:712_1
- RFN: 43245
- Chip: 6400
- Event: Start Timer
- Source: ts_RRC_Delay LINE 1
- Message Structure:
no details available
- Constraint:
t_Dly (1000 Ms)
- BinaryMessage:

- No.: 2578
- Timestamp: 17:23:54:710_0
- RFN: 43344
- Chip: 38144
- Event: Timeout
- Source: ts_RRC_Delay LINE 2
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 2583
- Timestamp: 17:23:54:711_0
- RFN: 43345
- Chip: 4608
- Event: Send
- PCO: UM
- Message: RLC_UM_DATA_REQ
- Source: ts_RRC_ConnRel:lt_Send_RRC_ConnectionRelease LINE 3
- Message Structure:
RLC_UM_DATA_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 1
. uM_message
. . DL_DCCH_Message
. . . IntegrityCheckInfo
. . . DL_DCCH_MessageType
. . . . RRCConnectionRelease
. . . . . r3
. . . . . . RRCConnectionRelease_r3_IEs
. . . . . . . (IntegerType)rrc_TransactionIdentifier[-1] = 0
. . . . . . . (IntegerType)n_308[-1] = 1
. . . . . . . (ReleaseCause)releaseCause[0] = 0
. . . . . . . Rplmn_Information
. . . . . . laterNonCriticalExtensions
. (BooleanType)specialLI = FALSE
- Constraint:
cas_RRC_ConnRelDCCH
- BinaryMessage:
30 0c 02 01 ff 02 01 01 3c 80 00 01 01 00

- No.: 2587
- Timestamp: 17:23:54:838_0
- RFN: 43357
- Chip: 29952
- Event: Receive
- PCO: UM
- Message: RLC_UM_DATA_IND
- Source: ts_RRC_ConnRel:lt_Send_RRC_ConnectionRelease LINE 4
- Message Structure:
RLC_UM_DATA_IND
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 1
. IntegrityResult
. uM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . UL_DCCH_MessageType
. . . . RRCConnectionReleaseComplete
. . . . . (IntegerType)rrc_TransactionIdentifier[2] = 0
. . . . . FailureCauseWithProtErr
. . . . . laterNonCriticalExtensions
- Constraint:
car_RRC_ConnRelCmplUM
- BinaryMessage:
30 0a 02 01 ff 02 01 01 05 00 44 00

- No.: 2588
- Timestamp: 17:23:54:839_0
- RFN: 43357
- Chip: 31232
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ConnRel:lt_Send_RRC_ConnectionRelease LINE 4
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2591
- Timestamp: 17:23:54:839_3
- RFN: 43357
- Chip: 33280
- Event: Start Timer
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 1
- Message Structure:
no details available
- Constraint:
t_Dly (5000 Ms)
- BinaryMessage:

- No.: 2595
- Timestamp: 17:23:54:998_0
- RFN: 43373
- Chip: 29952
- Event: Receive
- PCO: UM
- Message: RLC_UM_DATA_IND
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 4
- Message Structure:
RLC_UM_DATA_IND
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 1
. IntegrityResult
. uM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . UL_DCCH_MessageType
. . . . RRCConnectionReleaseComplete
. . . . . (IntegerType)rrc_TransactionIdentifier[2] = 0
. . . . . FailureCauseWithProtErr
. . . . . laterNonCriticalExtensions
- Constraint:
car_RRC_ConnRelCmplUM
- BinaryMessage:
30 08 02 01 ff 02 01 01 44 00

- No.: 2596
- Timestamp: 17:23:54:998_1
- RFN: 43373
- Chip: 31488
- Event: Cancel Timer
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 4
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 2597
- Timestamp: 17:23:54:998_2
- RFN: 43373
- Chip: 31744
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 4
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2603
- Timestamp: 17:23:54:999_3
- RFN: 43373
- Chip: 36352
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 1
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 01 0a 01 00 05 00

- No.: 2607
- Timestamp: 17:23:55:005_0
- RFN: 43374
- Chip: 21504
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 2610
- Timestamp: 17:23:55:006_2
- RFN: 43374
- Chip: 24832
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 2
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 02 0a 01 00 05 00

- No.: 2614
- Timestamp: 17:23:55:010_0
- RFN: 43375
- Chip: 2304
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 2617
- Timestamp: 17:23:55:011_2
- RFN: 43375
- Chip: 6144
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 3
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 03 0a 01 00 05 00

- No.: 2621
- Timestamp: 17:23:55:016_0
- RFN: 43375
- Chip: 25344
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 3
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 2624
- Timestamp: 17:23:55:017_2
- RFN: 43375
- Chip: 28672
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 4
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 04 0a 01 00 05 00

- No.: 2628
- Timestamp: 17:23:55:024_0
- RFN: 43376
- Chip: 15872
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 4
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 2631
- Timestamp: 17:23:55:025_0
- RFN: 43376
- Chip: 21504
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 1
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 136
. . . . . UL_RLC_Mode
. . . . . . UL_UM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (NoExplicitDiscard)timerBasedNoExplicit[0] = 9
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 1
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 1
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_UM_Info
- BinaryMessage:
30 22 02 01 ff 02 01 01 0a 01 00 30 17 30 0d 05 00 30 09 02 02 00 88 30 03 0a 01 09 30 06 02 01 01 02 01 01

- No.: 2635
- Timestamp: 17:23:55:030_0
- RFN: 43377
- Chip: 256
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 2636
- Timestamp: 17:23:55:031_0
- RFN: 43377
- Chip: 6656
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 3
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 2
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 2
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 2
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 02 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 13 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 02 02 01 02

- No.: 2640
- Timestamp: 17:23:55:040_0
- RFN: 43378
- Chip: 0
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 4
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 2641
- Timestamp: 17:23:55:041_0
- RFN: 43378
- Chip: 6400
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 5
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 3
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 3
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 3
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 03 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 13 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 03 02 01 03

- No.: 2645
- Timestamp: 17:23:55:050_0
- RFN: 43379
- Chip: 256
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 6
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 3
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 2646
- Timestamp: 17:23:55:052_0
- RFN: 43379
- Chip: 6912
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 7
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 4
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 4
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 4
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 04 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 13 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 04 02 01 04

- No.: 2650
- Timestamp: 17:23:55:060_0
- RFN: 43380
- Chip: 1536
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 8
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 4
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 2674
- Timestamp: 17:23:55:063_4
- RFN: 43380
- Chip: 13056
- Event: Start Timer
- Source: tc_12_4_1_4c2:lt_LocUpateStep8 LINE 2
- Message Structure:
no details available
- Constraint:
t_UpperBound (396000 Ms)
- BinaryMessage:

- No.: 2675
- Timestamp: 17:23:55:063_5
- RFN: 43380
- Chip: 13568
- Event: Start Timer
- Source: tc_12_4_1_4c2:lt_LocUpateStep8 LINE 2
- Message Structure:
no details available
- Constraint:
t_LowerBound (324000 Ms)
- BinaryMessage:

- No.: 2682
- Timestamp: 17:29:19:063_0
- RFN: 75783
- Chip: 4608
- Event: Timeout
- Source: tc_12_4_1_4c2:lt_LocUpateStep8 LINE 3
- Message Structure:
no details available
- Constraint:
t_LowerBound
- BinaryMessage:

- No.: 2686
- Timestamp: 17:29:54:408_0
- RFN: 79317
- Chip: 36096
- Event: Receive
- PCO: TM
- Message: RLC_TR_DATA_IND
- Source: tc_12_4_1_4c2:lt_LocUpateStep8 LINE 4
- Message Structure:
RLC_TR_DATA_IND
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 0
. tM_message
. . UL_CCCH_Message
. . . IntegrityCheckInfo
. . . UL_CCCH_MessageType
. . . . RRCConnectionRequest
. . . . . InitialUE_Identity
. . . . . . IMSI_GSM_MAP
. . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . (IntegerType)_elem[4] = 1
. . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . (IntegerType)_elem[4] = 1
. . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . (IntegerType)_elem[4] = 1
. . . . . . . (IntegerType)_elem[4] = 2
. . . . . . . (IntegerType)_elem[4] = 3
. . . . . . . (IntegerType)_elem[4] = 4
. . . . . . . (IntegerType)_elem[4] = 5
. . . . . . . (IntegerType)_elem[4] = 6
. . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . (IntegerType)_elem[4] = 6
. . . . . . . (IntegerType)_elem[4] = 3
. . . . . (EstablishmentCause)establishmentCause[5] = 12
. . . . . (ProtocolErrorIndicator)protocolErrorIndicator[1] = 0
. . . . . MeasuredResultsOnRACH
. . . . . v3d0NonCriticalExtensions
- Constraint:
car_RRC_ConnReq
- BinaryMessage:
30 10 02 01 00 02 01 00 20 90 01 01 01 23 45 60 63 60

- No.: 2687
- Timestamp: 17:29:54:409_0
- RFN: 79317
- Chip: 38144
- Event: Cancel Timer
- Source: tc_12_4_1_4c2:lt_LocUpateStep8 LINE 4
- Message Structure:
no details available
- Constraint:
t_UpperBound
- BinaryMessage:

- No.: 2688
- Timestamp: 17:29:54:409_1
- RFN: 79318
- Chip: 0
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: tc_12_4_1_4c2:lt_LocUpateStep8 LINE 4
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2703
- Timestamp: 17:29:54:420_0
- RFN: 79319
- Chip: 4608
- Event: Send
- PCO: UM
- Message: RLC_UM_DATA_REQ
- Source: ts_RRC_ConnEstEnd:lt_Send_ConnSetUp LINE 22
- Message Structure:
RLC_UM_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 0
. uM_message
. . DL_CCCH_Message
. . . IntegrityCheckInfo
. . . DL_CCCH_MessageType
. . . . RRCConnectionSetup
. . . . . r3
. . . . . . RRCConnectionSetup_r3_IEs
. . . . . . . InitialUE_Identity
. . . . . . . . IMSI_GSM_MAP
. . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . (IntegerType)_elem[4] = 1
. . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . (IntegerType)_elem[4] = 1
. . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . (IntegerType)_elem[4] = 1
. . . . . . . . . (IntegerType)_elem[4] = 2
. . . . . . . . . (IntegerType)_elem[4] = 3
. . . . . . . . . (IntegerType)_elem[4] = 4
. . . . . . . . . (IntegerType)_elem[4] = 5
. . . . . . . . . (IntegerType)_elem[4] = 6
. . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . (IntegerType)_elem[4] = 6
. . . . . . . . . (IntegerType)_elem[4] = 3
. . . . . . . (IntegerType)rrc_TransactionIdentifier[-1] = 0
. . . . . . . (IntegerType)activationTime[-1] = -
. . . . . . . U_RNTI
. . . . . . . . (BitStringType)srnc_Identity[12] = "000000000001"
. . . . . . . . (BitStringType)s_RNTI[20] = "00000000000000000001"
. . . . . . . (BitStringType)new_c_RNTI[16] = -
. . . . . . . (RRC_StateIndicator)rrc_StateIndicator[0] = 0
. . . . . . . (IntegerType)utran_DRX_CycleLengthCoeff[-1] = 9
. . . . . . . CapabilityUpdateRequirement
. . . . . . . . (BooleanType)ue_RadioCapabilityFDDUpdateRequirement = TRUE
. . . . . . . . (BooleanType)ue_RadioCapabilityTDDUpdateRequirement = FALSE
. . . . . . . . SystemSpecificCapUpdateReqList
. . . . . . . . . (SystemSpecificCapUpdateReq)_elem[0] = 0
. . . . . . . SRB_InformationSetupList2
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity[-1] = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_UM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 1
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex[-1] = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 1
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity[-1] = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 2
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 2
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 2
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 2
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex[-1] = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 2
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 2
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity[-1] = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 3
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 3
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 3
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 3
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex[-1] = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 3
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 3
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity[-1] = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 4
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 4
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 4
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 4
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex[-1] = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 4
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 4
. . . . . . . UL_CommonTransChInfo
. . . . . . . . TFC_Subset
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . TFCS
. . . . . . . . . . . ExplicitTFCS_Configuration
. . . . . . . . . . . . TFCS_ReconfAdd
. . . . . . . . . . . . . ctfcSize
. . . . . . . . . . . . . . ctfc2Bit
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . . . . . . . (IntegerType)ctfc2[-1] = 0
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . . . . . . . (IntegerType)ctfc2[-1] = 1
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC[-1] = 11
. . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaD[-1] = 15
. . . . . . . . . . . . . . . . . . . (IntegerType)referenceTFC_ID[-1] = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . UL_AddReconfTransChInfoList
. . . . . . . . UL_AddReconfTransChInformation
. . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType[0] = 0
. . . . . . . . . (IntegerType)transportChannelIdentity[-1] = 5
. . . . . . . . . TransportFormatSet
. . . . . . . . . . DedicatedTransChTFS
. . . . . . . . . . . tti
. . . . . . . . . . . . DedicatedDynamicTF_InfoList
. . . . . . . . . . . . . DedicatedDynamicTF_Info
. . . . . . . . . . . . . . rlc_Size
. . . . . . . . . . . . . . . BitModeRLC_SizeInfo
. . . . . . . . . . . . . . . . sizeType2
. . . . . . . . . . . . . . . . . (IntegerType)part1[-1] = 2
. . . . . . . . . . . . . . . . . (IntegerType)part2[-1] = -
. . . . . . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . LogicalChannelList
. . . . . . . . . . . SemistaticTF_Information
. . . . . . . . . . . . ChannelCodingType
. . . . . . . . . . . . . (CodingRate)convolutional[0] = 1
. . . . . . . . . . . . (IntegerType)rateMatchingAttribute[-1] = 192
. . . . . . . . . . . . (CRC_Size)crc_Size[0] = 3
. . . . . . . DL_CommonTransChInfo
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . dl_Parameters
. . . . . . . DL_AddReconfTransChInfoList
. . . . . . . . DL_AddReconfTransChInformation
. . . . . . . . . (DL_TrCH_Type)dl_TransportChannelType[0] = 0
. . . . . . . . . (IntegerType)dl_transportChannelIdentity[-1] = 10
. . . . . . . . . tfs_SignallingMode
. . . . . . . . . . UL_TransportChannelIdentity
. . . . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType[0] = 0
. . . . . . . . . . . (IntegerType)ul_TransportChannelIdentity[-1] = 5
. . . . . . . . . QualityTarget
. . . . . . . . . . (IntegerType)bler_QualityValue[-1] = -20
. . . . . . . . . TM_SignallingInfo
. . . . . . . FrequencyInfo
. . . . . . . (IntegerType)maxAllowedUL_TX_Power[-1] = -
. . . . . . . UL_ChannelRequirement
. . . . . . . . UL_DPCH_Info
. . . . . . . . . UL_DPCH_PowerControlInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (IntegerType)dpcch_PowerOffset[-1] = -40
. . . . . . . . . . . (IntegerType)pc_Preamble[-1] = 1
. . . . . . . . . . . (IntegerType)sRB_delay[-1] = 7
. . . . . . . . . . . PowerControlAlgorithm
. . . . . . . . . . . . (IntegerType)algorithm1[-1] = 1
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (ScramblingCodeType)scramblingCodeType[0] = 1
. . . . . . . . . . . (IntegerType)scramblingCode[-1] = 0
. . . . . . . . . . . (IntegerType)numberOfDPDCH[-1] = -
. . . . . . . . . . . (SpreadingFactor)spreadingFactor[0] = 4
. . . . . . . . . . . (BooleanType)tfci_Existence = TRUE
. . . . . . . . . . . (IntegerType)numberOfFBI_Bits[-1] = -
. . . . . . . . . . . (PuncturingLimit)puncturingLimit[0] = 15
. . . . . . . DL_CommonInformation
. . . . . . . . DL_DPCH_InfoCommon
. . . . . . . . . cfnHandling
. . . . . . . . . . initialise
. . . . . . . . . . . (IntegerType)cfntargetsfnframeoffset[-1] = -
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . DL_DPCH_PowerControlInfo
. . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . (DPC_Mode)dpc_Mode[0] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPilot_pdpdch[-1] = 0
. . . . . . . . . . . Dl_rate_matching_restriction
. . . . . . . . . . . SF512_AndPilot
. . . . . . . . . . . . (PilotBits128)sfd128[0] = 0
. . . . . . . . . . . (PositionFixedOrFlexible)positionFixedOrFlexible[0] = 0
. . . . . . . . . . . (BooleanType)tfci_Existence = FALSE
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . (IntegerType)defaultDPCH_OffsetValue[-1] = 459
. . . . . . . . . . DPCH_CompressedModeInfo
. . . . . . . . . . (TX_DiversityMode)tx_DiversityMode[0] = 0
. . . . . . . . . . SSDT_Information
. . . . . . . DL_InformationPerRL_List
. . . . . . . . DL_InformationPerRL
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . PrimaryCPICH_Info
. . . . . . . . . . . . (IntegerType)primaryScramblingCode[-1] = 100
. . . . . . . . . . . PDSCH_SHO_DCH_Info
. . . . . . . . . . . PDSCH_CodeMapping
. . . . . . . . . DL_DPCH_InfoPerRL
. . . . . . . . . . fdd
. . . . . . . . . . . (PCPICH_UsageForChannelEst)pCPICH_UsageForChannelEst[0] = 0
. . . . . . . . . . . (IntegerType)dpch_FrameOffset[-1] = 18
. . . . . . . . . . . SecondaryCPICH_Info
. . . . . . . . . . . DL_ChannelisationCodeList
. . . . . . . . . . . . DL_ChannelisationCode
. . . . . . . . . . . . . (IntegerType)secondaryScramblingCode[-1] = 1
. . . . . . . . . . . . . SF512_AndCodeNumber
. . . . . . . . . . . . . . (IntegerType)sf128[-1] = 0
. . . . . . . . . . . . . (ScramblingCodeChange)scramblingCodeChange[0] = 1
. . . . . . . . . . . (IntegerType)tpc_CombinationIndex[-1] = 0
. . . . . . . . . . . (SSDT_CellIdentity)ssdt_CellIdentity[0] = -
. . . . . . . . . . . (ClosedLoopTimingAdjMode)closedLoopTimingAdjMode[0] = -
. . . . . . . . . SCCPCH_InfoForFACH
. . . . . . laterNonCriticalExtensions
. (BooleanType)specialLI = TRUE
- Constraint:
cas_RRC_ConnSetup
- BinaryMessage:
30 78 02 01 00 02 01 00 30 e7 12 00 20 20 24 68 ac 0c 60 00 80 00 09 b0 4d 27 42 02 11 21 a8 40 00 50 33 d1 c8 d9 34 cf 93 89 ce 84 14 a2 47 51 80 02 a2 67 a3 91 b2 69 9f 27 13 9d 08 4a 44 96 a5 00 09 48 cf 47 23 64 d3 3e 4e 27 3a 10 d6 89 3d 4e 00 1a 99 00 00 c4 a5 7e 00 40 01 10 44 77 ec c1 13 12 b4 a8 f4 40 00 00 27 f2 01 42 9c b0 40 c8 01 21 85 01 00 01 01 ff

- No.: 2724
- Timestamp: 17:29:54:442_7
- RFN: 79321
- Chip: 14336
- Event: Start Timer
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 3
- Message Structure:
no details available
- Constraint:
t_WaitMS (13500 Ms)
- BinaryMessage:

- No.: 2726
- Timestamp: 17:29:54:443_1
- RFN: 79321
- Chip: 16128
- Event: Receive
- PCO: CPHY
- Message: CPHY_Out_of_Sync_IND
- Source: RRC_DefConnEst LINE 7
- Message Structure:
CPHY_Out_of_Sync_IND
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 20
- Constraint:
ca_OutOfSyncInd
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 2727
- Timestamp: 17:29:54:443_2
- RFN: 79321
- Chip: 17152
- Event: Cancel Timer
- Source: RRC_DefConnEst LINE 7
- Message Structure:
no details available
- Constraint:
t_T312
- BinaryMessage:

- No.: 2728
- Timestamp: 17:29:54:443_3
- RFN: 79321
- Chip: 17664
- Event: Default
- Source: RRC_DefConnEst LINE 0
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2729
- Timestamp: 17:29:54:443_4
- RFN: 79321
- Chip: 18176
- Event: Default
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2737
- Timestamp: 17:29:54:656_1
- RFN: 79342
- Chip: 29952
- Event: Receive
- PCO: CPHY
- Message: CPHY_Sync_IND
- Source: RRC_DefConnEst LINE 5
- Message Structure:
CPHY_Sync_IND
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 20
- Constraint:
ca_SyncInd
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 2738
- Timestamp: 17:29:54:656_2
- RFN: 79342
- Chip: 30720
- Event: Cancel Timer
- Source: RRC_DefConnEst LINE 5
- Message Structure:
no details available
- Constraint:
t_T312
- BinaryMessage:

- No.: 2739
- Timestamp: 17:29:54:656_3
- RFN: 79342
- Chip: 31488
- Event: Default
- Source: RRC_DefConnEst LINE 0
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2740
- Timestamp: 17:29:54:656_4
- RFN: 79342
- Chip: 31744
- Event: Default
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2747
- Timestamp: 17:29:54:758_0
- RFN: 79352
- Chip: 35072
- Event: Receive
- PCO: AM
- Message: RLC_AM_DATA_IND
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
RLC_AM_DATA_IND
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 2
. IntegrityResult
. . (IntegrityStatus)integrityUsed[0] = 4294967296
. aM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . UL_DCCH_MessageType
. . . . RRCConnectionSetupComplete
. . . . . (IntegerType)rrc_TransactionIdentifier[2] = 0
. . . . . STARTList
. . . . . . STARTSingle
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity[1] = 1
. . . . . . . (BitStringType)start_Value[20] = "00000000000000000010"
. . . . . . STARTSingle
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity[1] = 0
. . . . . . . (BitStringType)start_Value[20] = "00000000000000000010"
. . . . . UE_RadioAccessCapability
. . . . . . (AccessStratumReleaseIndicator)accessStratumReleaseIndicator[0] = 0
. . . . . . PDCP_Capability
. . . . . . . (BooleanType)losslessSRNS_RelocationSupport = FALSE
. . . . . . . supportForRfc2507
. . . . . . . . (MaxHcContextSpace)supported[3] = 4
. . . . . . RLC_Capability
. . . . . . . (TotalRLC_AM_BufferSize)totalRLC_AM_BufferSize[3] = 2
. . . . . . . (MaximumRLC_WindowSize)maximumRLC_WindowSize[1] = 0
. . . . . . . (MaximumAM_EntityNumberRLC_Cap)maximumAM_EntityNumber[3] = 3
. . . . . . TransportChannelCapability
. . . . . . . DL_TransChCapability
. . . . . . . . (MaxNoBits)maxNoBitsReceived[4] = 7
. . . . . . . . (MaxNoBits)maxConvCodeBitsReceived[4] = 1
. . . . . . . . TurboSupport
. . . . . . . . . (MaxNoBits)supported[4] = 7
. . . . . . . . (MaxSimultaneousTransChsDL)maxSimultaneousTransChs[2] = 1
. . . . . . . . (IntegerType)maxSimultaneousCCTrCH_Count[3] = 1
. . . . . . . . (MaxTransportBlocksDL)maxReceivedTransportBlocks[4] = 3
. . . . . . . . (MaxNumberOfTFC_DL)maxNumberOfTFC[4] = 5
. . . . . . . . (MaxNumberOfTF)maxNumberOfTF[3] = 1
. . . . . . . UL_TransChCapability
. . . . . . . . (MaxNoBits)maxNoBitsTransmitted[4] = 3
. . . . . . . . (MaxNoBits)maxConvCodeBitsTransmitted[4] = 1
. . . . . . . . TurboSupport
. . . . . . . . . (MaxNoBits)supported[4] = 3
. . . . . . . . (MaxSimultaneousTransChsUL)maxSimultaneousTransChs[3] = 2
. . . . . . . . modeSpecificInfo
. . . . . . . . (MaxTransportBlocksUL)maxTransmittedBlocks[4] = 4
. . . . . . . . (MaxNumberOfTFC_UL)maxNumberOfTFC[4] = 5
. . . . . . . . (MaxNumberOfTF)maxNumberOfTF[3] = 0
. . . . . . RF_Capability
. . . . . . . fddRF_Capability
. . . . . . . . (IntegerType)ue_PowerClass[2] = 4
. . . . . . . . (TxRxFrequencySeparation)txRxFrequencySeparation[2] = 0
. . . . . . . tddRF_Capability
. . . . . . PhysicalChannelCapability
. . . . . . . fddPhysChCapability
. . . . . . . . DL_PhysChCapabilityFDD
. . . . . . . . . (IntegerType)maxNoDPCH_PDSCH_Codes[3] = 1
. . . . . . . . . (MaxNoPhysChBitsReceived)maxNoPhysChBitsReceived[4] = 6
. . . . . . . . . (BooleanType)supportForSF_512 = FALSE
. . . . . . . . . (BooleanType)supportOfPDSCH = FALSE
. . . . . . . . . SimultaneousSCCPCH_DPCH_Reception
. . . . . . . . UL_PhysChCapabilityFDD
. . . . . . . . . (MaxNoDPDCH_BitsTransmitted)maxNoDPDCH_BitsTransmitted[4] = 3
. . . . . . . . . (BooleanType)supportOfPCPCH = FALSE
. . . . . . . tddPhysChCapability
. . . . . . UE_MultiModeRAT_Capability
. . . . . . . MultiRAT_Capability
. . . . . . . . (BooleanType)supportOfGSM = FALSE
. . . . . . . . (BooleanType)supportOfMulticarrier = FALSE
. . . . . . . (MultiModeCapability)multiModeCapability[2] = 1
. . . . . . SecurityCapability
. . . . . . . (BitStringType)cipheringAlgorithmCap[16] = '0000000000000011'B
. . . . . . . (BitStringType)integrityProtectionAlgorithmCap[16] = '0000000000000010'B
. . . . . . UE_Positioning_Capability
. . . . . . . (BooleanType)standaloneLocMethodsSupported = FALSE
. . . . . . . (BooleanType)ue_BasedOTDOA_Supported = FALSE
. . . . . . . (NetworkAssistedGPS_Supported)networkAssistedGPS_Supported[2] = 3
. . . . . . . (BooleanType)supportForUE_GPS_TimingOfCellFrames = FALSE
. . . . . . . (BooleanType)supportForIPDL = FALSE
. . . . . . MeasurementCapability
. . . . . . . CompressedModeMeasCapability
. . . . . . . . (BooleanType)fdd_Measurements = TRUE
. . . . . . . . (BooleanType)tdd_Measurements = -
. . . . . . . . GSM_Measurements
. . . . . . . . . (BooleanType)gsm900 = TRUE
. . . . . . . . . (BooleanType)dcs1800 = TRUE
. . . . . . . . . (BooleanType)gsm1900 = TRUE
. . . . . . . . (BooleanType)multiCarrierMeasurements = FALSE
. . . . . . . CompressedModeMeasCapability
. . . . . . . . (BooleanType)fdd_Measurements = TRUE
. . . . . . . . (BooleanType)tdd_Measurements = -
. . . . . . . . GSM_Measurements
. . . . . . . . . (BooleanType)gsm900 = TRUE
. . . . . . . . . (BooleanType)dcs1800 = TRUE
. . . . . . . . . (BooleanType)gsm1900 = TRUE
. . . . . . . . (BooleanType)multiCarrierMeasurements = FALSE
. . . . . v370NonCriticalExtensions
- Constraint:
car_RRC_ConnSetupCmpl
- BinaryMessage:
30 27 02 01 ff 02 01 02 0a 05 01 00 00 00 00 4a 0c 00 00 80 00 05 62 37 1b a0 d4 98 cd 11 45 90 60 61 00 03 00 02 31 f9 f8

- No.: 2748
- Timestamp: 17:29:54:759_0
- RFN: 79353
- Chip: 3328
- Event: Cancel Timer
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
t_WaitMS
- BinaryMessage:

- No.: 2749
- Timestamp: 17:29:54:760_0
- RFN: 79353
- Chip: 3584
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2767
- Timestamp: 17:29:54:777_0
- RFN: 79354
- Chip: 30720
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: tc_12_4_1_4c2:lt_LocUpateStep8 LINE 6
- Message Structure:
RRC_DataInd
. (IntegerType)cellId[0] = -1
. (SS_RB_Identity)rB_Id[0] = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain[0] = 0
. (START_Value)start[20] = '00000000000000000010'B
. LOCATIONUPDATINGREQUEST
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)mMProtocolDiscriminator[4] = '0101'B
. . (MsgType)msgType[8] = '00001000'B
. . CiphKeySeqNum
. . . (B1)spare1[1] = '0'B
. . . (KeySeq)keySeq[3] = '001'B
. . LocUpdType
. . . (B1)fOR[1] = '0'B
. . . (B1)spare1[1] = '0'B
. . . (B2)lUT[2] = '01'B
. . LocAreaId_v
. . . (OctetStringType)plmn[3] = '00F110'O
. . . (OctetStringType)lac[2] = '0001'O
. . MS_Clsmk1
. . . (B1)spare1[1] = '0'B
. . . (B2)revLvl[2] = '10'B
. . . (B1)eSIND[1] = '0'B
. . . (B1)a5_1[1] = '1'B
. . . (B3)rFPwrCap[3] = '111'B
. . MS_Identity_lv
. . . (Length)iel[1] = '08'O
. . . (B4)iDigit1[4] = '0000'B
. . . (B1)oddEvenInd[1] = '1'B
. . . (B3)typeOfId[3] = '001'B
. . . (OctetStringType)otherDigits[7] = '10101032540636'O
. . MS_Clsmk2
. . . (IEI8)iei[8] = '00110011'B
. . . (Length)iel[1] = '03'O
. . . (B1)spare1_1[1] = '0'B
. . . (B2)revLvl[2] = '10'B
. . . (B1)eSIND[1] = '0'B
. . . (B1)a5_1[1] = '1'B
. . . (B3)rFPwrCap[3] = '111'B
. . . (B1)spare1_2[1] = '0'B
. . . (B1)pSCap[1] = '0'B
. . . (B2)sSSI[2] = '01'B
. . . (B1)sMCap[1] = '1'B
. . . (B1)vBS[1] = '0'B
. . . (B1)vGCS[1] = '0'B
. . . (B1)fC[1] = '0'B
. . . (B1)cM3[1] = '1'B
. . . (B1)spare1_3[1] = '0'B
. . . (B1)lCSVA[1] = '1'B
. . . (B1)uCS2[1] = '0'B
. . . (B1)soLSA[1] = '0'B
. . . (B1)cMSP[1] = '0'B
. . . (B1)a5_3[1] = '0'B
. . . (B1)a5_2[1] = '0'B
- Constraint:
car_InitDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 00 03 04 04 00 00 20 05 08 11 00 f1 10 00 01 4f 08 09 10 10 10 32 54 06 36 33 03 4f 18 a0

- No.: 2803
- Timestamp: 17:29:54:783_0
- RFN: 79355
- Chip: 15360
- Event: Send
- PCO: Dc
- Message: RRC_DataReq
- Source: ts_MM_Authentication LINE 2
- Message Structure:
RRC_DataReq
. (IntegerType)cellId[-1] = -1
. (SS_RB_Identity)rB_Id[-1] = 3
. (LogicChGERAN)ch[-1] = -
. (SapId)sapId[1] = -
. (SS_CN_DomainIdentity)cN_Domain[-1] = 0
. AUTHENTICATIONREQUEST
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)mMProtocolDiscriminator[4] = '0101'B
. . (MsgType)msgType[8] = '00010010'B
. . (B4)spare4[4] = '0000'B
. . CiphKeySeqNum
. . . (B1)spare1[1] = '0'B
. . . (KeySeq)keySeq[3] = '010'B
. . (MM_RAND)rAND[128] = '01010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101'B
. . AUTN
. . . (IEI8)iei[8] = '00100000'B
. . . (Length)iel[1] = '10'O
. . . (BitStringType)aUTN[128] = '01010110010100010101000001010011010100100101110100000000000000000101010101010100010101110101011001010001010100000101001101010010'B
- Constraint:
ca_DataReq
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 00 05 12 02 55 55 55 55 55 55 55 55 55 55 55 55 55 55 55 55 20 10 56 51 50 53 52 5d 00 00 55 54 57 56 51 50 53 52

- No.: 2807
- Timestamp: 17:29:55:056_0
- RFN: 79382
- Chip: 28928
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_MM_Authentication LINE 3
- Message Structure:
RRC_DataInd
. (IntegerType)cellId[0] = -1
. (SS_RB_Identity)rB_Id[0] = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain[0] = 0
. (START_Value)start[0] = -
. AUTHENTICATIONRESPONSE
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)mMProtocolDiscriminator[4] = '0101'B
. . (MsgType)msgType[8] = '01010100'B
. . (AuthRsp)authRsp[32] = '01010101010101000101011101010110'B
. . AuthRspExt
. . . (IEI8)iei[8] = '00100001'B
. . . (Length)iel[1] = '0C'O
. . . (BitStringType)rES[96] = '010100010101000001010011010100100101110101011100010111110101111001011001010110000101101101011010'B
- Constraint:
car_UplinkDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 00 05 54 55 54 57 56 21 0c 51 50 53 52 5d 5c 5f 5e 59 58 5b 5a

- No.: 2849
- Timestamp: 17:29:55:062_0
- RFN: 79383
- Chip: 12800
- Event: Send
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_REQ
- Source: ts_SS_DownloadSecurityKey:lt_DownloadKeyCRLC LINE 1
- Message Structure:
CRLC_SecurityMode_Config_REQ
. (IntegerType)cellId[-1] = -1
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity[0] = 0
. . (BitStringType)startValue[20] = "00000000000000000000"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = '01010111010101100101000101010000010100110101001001011101010111000101111101011110010110010101100001011011010110100101010101010100'B
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CRLC_SecurityModeCfgReq
- BinaryMessage:
30 21 02 01 ff 30 1c 0a 01 00 03 04 04 00 00 00 03 11 00 57 56 51 50 53 52 5d 5c 5f 5e 59 58 5b 5a 55 54

- No.: 2850
- Timestamp: 17:29:55:062_1
- RFN: 79383
- Chip: 14336
- Event: Receive
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_CNF
- Source: ts_SS_DownloadSecurityKey:lt_DownloadKeyCRLC LINE 2
- Message Structure:
CRLC_SecurityMode_Config_CNF
. (IntegerType)cellId[0] = -1
- Constraint:
ca_CRLC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 2857
- Timestamp: 17:29:55:063_6
- RFN: 79383
- Chip: 18688
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 1
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 0
. (IntegerType)count_I_LSB_UL[-1] = -
. (IntegerType)count_I_LSB_DL[-1] = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 00 02 01 00 02 01 00

- No.: 2858
- Timestamp: 17:29:55:064_0
- RFN: 79383
- Chip: 20480
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 2
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 0
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 00 02 01 00

- No.: 2859
- Timestamp: 17:29:55:064_1
- RFN: 79383
- Chip: 22272
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 3
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 1
. (IntegerType)count_I_LSB_UL[-1] = -
. (IntegerType)count_I_LSB_DL[-1] = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 01 02 01 00

- No.: 2860
- Timestamp: 17:29:55:065_0
- RFN: 79383
- Chip: 23808
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 4
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 1
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 2861
- Timestamp: 17:29:55:065_1
- RFN: 79383
- Chip: 25600
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 5
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 2
. (IntegerType)count_I_LSB_UL[-1] = -
. (IntegerType)count_I_LSB_DL[-1] = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 02 02 01 00

- No.: 2862
- Timestamp: 17:29:55:066_0
- RFN: 79383
- Chip: 27136
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 6
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 2
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 2863
- Timestamp: 17:29:55:066_1
- RFN: 79383
- Chip: 29184
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 7
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 3
. (IntegerType)count_I_LSB_UL[-1] = -
. (IntegerType)count_I_LSB_DL[-1] = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 03 02 01 00

- No.: 2864
- Timestamp: 17:29:55:067_0
- RFN: 79383
- Chip: 30976
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 8
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 3
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 2865
- Timestamp: 17:29:55:067_1
- RFN: 79383
- Chip: 33280
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 9
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 4
. (IntegerType)count_I_LSB_UL[-1] = -
. (IntegerType)count_I_LSB_DL[-1] = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 04 02 01 00

- No.: 2866
- Timestamp: 17:29:55:068_0
- RFN: 79383
- Chip: 34816
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 10
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 4
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 2870
- Timestamp: 17:29:55:069_0
- RFN: 79384
- Chip: 768
- Event: Send
- PCO: CRLC
- Message: CRLC_Integrity_Activate_REQ
- Source: ts_CRLC_DL_Integrity LINE 1
- Message Structure:
CRLC_Integrity_Activate_REQ
. (IntegerType)cellId[-1] = -1
. (CN_DomainIdentity)cn_DomainIdentity[0] = 0
. IntegrityActivationInfo
. . IntegrityProtectionModeInfo
. . . IntegrityProtectionModeCommand
. . . . startIntegrityProtection
. . . . . (BitStringType)integrityProtInitNumber[32] = "00000000000000000000000000000001"
. . . (IntegrityProtectionAlgorithm)integrityProtectionAlgorithm[0] = 0
- Constraint:
ca_CRLC_DL_IntegrityActivateReq
- BinaryMessage:
30 14 02 01 ff 0a 01 00 30 0c 30 07 03 05 00 00 00 00 01 0a 01 00

- No.: 2871
- Timestamp: 17:29:55:069_1
- RFN: 79384
- Chip: 2816
- Event: Receive
- PCO: CRLC
- Message: CRLC_Integrity_Activate_CNF
- Source: ts_CRLC_DL_Integrity LINE 2
- Message Structure:
CRLC_Integrity_Activate_CNF
. (IntegerType)cellId[0] = -1
- Constraint:
ca_CRLC_IntegrityActivateCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 2878
- Timestamp: 17:29:55:071_0
- RFN: 79384
- Chip: 7936
- Event: Send
- PCO: CRLC
- Message: CRLC_Integrity_Activate_REQ
- Source: ts_RB2_UL_IntegrityActivate LINE 1
- Message Structure:
CRLC_Integrity_Activate_REQ
. (IntegerType)cellId[-1] = -1
. (CN_DomainIdentity)cn_DomainIdentity[0] = 0
. IntegrityActivationInfo
. . IntegrityProtActivationInfoList
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity[-1] = 2
. . . . (IntegerType)rrc_MessageSequenceNumber[-1] = 0
- Constraint:
ca_CRLC_UL_IntegrityActivateReq
- BinaryMessage:
30 10 02 01 ff 0a 01 00 30 08 30 06 02 01 02 02 01 00

- No.: 2879
- Timestamp: 17:29:55:071_1
- RFN: 79384
- Chip: 9984
- Event: Receive
- PCO: CRLC
- Message: CRLC_Integrity_Activate_CNF
- Source: ts_RB2_UL_IntegrityActivate LINE 2
- Message Structure:
CRLC_Integrity_Activate_CNF
. (IntegerType)cellId[0] = -1
- Constraint:
ca_CRLC_IntegrityActivateCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 2886
- Timestamp: 17:29:55:073_0
- RFN: 79384
- Chip: 16384
- Event: Send
- PCO: AM
- Message: RLC_AM_DATA_REQ
- Source: ts_RRC_Security:lt_SendSecurityModeCommand LINE 16
- Message Structure:
RLC_AM_DATA_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 2
. AmConfirmationRequest
. aM_message
. . DL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00000000000000000000000000000000"
. . . . (IntegerType)rrc_MessageSequenceNumber[-1] = 0
. . . DL_DCCH_MessageType
. . . . SecurityModeCommand
. . . . . r3
. . . . . . SecurityModeCommand_r3_IEs
. . . . . . . (IntegerType)rrc_TransactionIdentifier[-1] = 0
. . . . . . . SecurityCapability
. . . . . . . . (BitStringType)cipheringAlgorithmCap[16] = '0000000000000011'B
. . . . . . . . (BitStringType)integrityProtectionAlgorithmCap[16] = '0000000000000010'B
. . . . . . . CipheringModeInfo
. . . . . . . IntegrityProtectionModeInfo
. . . . . . . . IntegrityProtectionModeCommand
. . . . . . . . . startIntegrityProtection
. . . . . . . . . . (BitStringType)integrityProtInitNumber[32] = "00000000000000000000000000000001"
. . . . . . . . (IntegrityProtectionAlgorithm)integrityProtectionAlgorithm[0] = 0
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity[0] = 0
. . . . . . . InterRAT_UE_SecurityCapList
. . . . . . laterNonCriticalExtensions
- Constraint:
cas_RRC_SecModeCmd
- BinaryMessage:
30 17 02 01 ff 02 01 02 05 00 80 00 00 00 04 04 00 01 80 01 40 00 00 00 20

- No.: 2895
- Timestamp: 17:29:55:196_0
- RFN: 79396
- Chip: 30464
- Event: Receive
- PCO: AM
- Message: RLC_AM_DATA_IND
- Source: ts_RRC_Security:lt_StartSecurity_UE LINE 8
- Message Structure:
RLC_AM_DATA_IND
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 2
. IntegrityResult
. . (IntegrityStatus)integrityUsed[0] = 0
. aM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "10000001100000001110110111011101"
. . . . (IntegerType)rrc_MessageSequenceNumber[4] = 1
. . . UL_DCCH_MessageType
. . . . SecurityModeComplete
. . . . . (IntegerType)rrc_TransactionIdentifier[2] = 0
. . . . . IntegrityProtActivationInfo
. . . . . . RRC_MessageSequenceNumberList
. . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . (IntegerType)_elem[4] = 0
. . . . . laterNonCriticalExtensions
- Constraint:
car_RRC_SecModeCmpl
- BinaryMessage:
30 12 02 01 ff 02 01 02 0a 01 00 c0 c0 76 ee 8d 21 00 00 00

- No.: 2896
- Timestamp: 17:29:55:197_0
- RFN: 79396
- Chip: 32000
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_Security:lt_StartSecurity_UE LINE 8
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2898
- Timestamp: 17:29:55:197_2
- RFN: 79396
- Chip: 35072
- Event: Send
- PCO: CRLC
- Message: CRLC_Integrity_Activate_REQ
- Source: ts_CRLC_UL_Integrity LINE 1
- Message Structure:
CRLC_Integrity_Activate_REQ
. (IntegerType)cellId[-1] = -1
. (CN_DomainIdentity)cn_DomainIdentity[0] = 0
. IntegrityActivationInfo
. . IntegrityProtActivationInfoList
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity[-1] = 0
. . . . (IntegerType)rrc_MessageSequenceNumber[-1] = 0
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity[-1] = 1
. . . . (IntegerType)rrc_MessageSequenceNumber[-1] = 0
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity[-1] = 3
. . . . (IntegerType)rrc_MessageSequenceNumber[-1] = 0
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity[-1] = 4
. . . . (IntegerType)rrc_MessageSequenceNumber[-1] = 0
- Constraint:
ca_CRLC_UL_IntegrityActivateReq
- BinaryMessage:
30 28 02 01 ff 0a 01 00 30 20 30 06 02 01 00 02 01 00 30 06 02 01 01 02 01 00 30 06 02 01 03 02 01 00 30 06 02 01 04 02 01 00

- No.: 2899
- Timestamp: 17:29:55:198_0
- RFN: 79396
- Chip: 37120
- Event: Receive
- PCO: CRLC
- Message: CRLC_Integrity_Activate_CNF
- Source: ts_CRLC_UL_Integrity LINE 2
- Message Structure:
CRLC_Integrity_Activate_CNF
. (IntegerType)cellId[0] = -1
- Constraint:
ca_CRLC_IntegrityActivateCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 2904
- Timestamp: 17:29:55:199_0
- RFN: 79397
- Chip: 3840
- Event: Send
- PCO: Dc
- Message: RRC_DataReq
- Source: tc_12_4_1_4c2:lt_LocUpateStep8 LINE 10
- Message Structure:
RRC_DataReq
. (IntegerType)cellId[-1] = -1
. (SS_RB_Identity)rB_Id[-1] = 3
. (LogicChGERAN)ch[-1] = -
. (SapId)sapId[1] = -
. (SS_CN_DomainIdentity)cN_Domain[-1] = 0
. LOCATIONUPDATINGACCEPT
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)mMProtocolDiscriminator[4] = '0101'B
. . (MsgType)msgType[8] = '00000010'B
. . LocAreaId_v
. . . (OctetStringType)plmn[3] = '00F110'O
. . . (OctetStringType)lac[2] = '0001'O
. . MM_MS_Identity
. . . (IEI8)iei[8] = '00010111'B
. . . (Length)iel[1] = '05'O
. . . (B4)iDigit1[4] = '1111'B
. . . (B1)oddEvenInd[1] = '0'B
. . . (B3)typeOfId[3] = '100'B
. . . (OctetStringType)otherDigits[-1] = '12345678'O
. . (FollowOnProceed)followOnProceed[8] = '10100001'B
. . (CTSPerm)cTSPerm[8] = '10100010'B
. . PLMN_List
- Constraint:
ca_DataReq
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 00 05 02 00 f1 10 00 01 17 05 f4 12 34 56 78 a1 a2

- No.: 2911
- Timestamp: 17:29:55:336_0
- RFN: 79410
- Chip: 28672
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: tc_12_4_1_4c2:lt_LocUpateStep8 LINE 11
- Message Structure:
RRC_DataInd
. (IntegerType)cellId[0] = -1
. (SS_RB_Identity)rB_Id[0] = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain[0] = 0
. (START_Value)start[0] = -
. TMSIREALLOCATIONCOMPLETE
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)mMProtocolDiscriminator[4] = '0101'B
. . (MsgType)msgType[8] = '10011011'B
- Constraint:
car_UplinkDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 00 05 9b

- No.: 2919
- Timestamp: 17:29:55:337_7
- RFN: 79410
- Chip: 33024
- Event: Start Timer
- Source: ts_RRC_Delay LINE 1
- Message Structure:
no details available
- Constraint:
t_Dly (1000 Ms)
- BinaryMessage:

- No.: 2923
- Timestamp: 17:29:56:327_0
- RFN: 79509
- Chip: 31744
- Event: Timeout
- Source: ts_RRC_Delay LINE 2
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 2928
- Timestamp: 17:29:56:328_0
- RFN: 79509
- Chip: 36864
- Event: Send
- PCO: UM
- Message: RLC_UM_DATA_REQ
- Source: ts_RRC_ConnRel:lt_Send_RRC_ConnectionRelease LINE 3
- Message Structure:
RLC_UM_DATA_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 1
. uM_message
. . DL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00000000000000000000000000000000"
. . . . (IntegerType)rrc_MessageSequenceNumber[-1] = 0
. . . DL_DCCH_MessageType
. . . . RRCConnectionRelease
. . . . . r3
. . . . . . RRCConnectionRelease_r3_IEs
. . . . . . . (IntegerType)rrc_TransactionIdentifier[-1] = 0
. . . . . . . (IntegerType)n_308[-1] = 1
. . . . . . . (ReleaseCause)releaseCause[0] = 0
. . . . . . . Rplmn_Information
. . . . . . laterNonCriticalExtensions
. (BooleanType)specialLI = FALSE
- Constraint:
cas_RRC_ConnRelDCCH
- BinaryMessage:
30 10 02 01 ff 02 01 01 80 00 00 00 03 c8 00 01 01 00

- No.: 2932
- Timestamp: 17:29:56:456_0
- RFN: 79522
- Chip: 29440
- Event: Receive
- PCO: UM
- Message: RLC_UM_DATA_IND
- Source: ts_RRC_ConnRel:lt_Send_RRC_ConnectionRelease LINE 4
- Message Structure:
RLC_UM_DATA_IND
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 1
. IntegrityResult
. uM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "10101101101011101001000000111001"
. . . . (IntegerType)rrc_MessageSequenceNumber[4] = 1
. . . UL_DCCH_MessageType
. . . . RRCConnectionReleaseComplete
. . . . . (IntegerType)rrc_TransactionIdentifier[2] = 0
. . . . . FailureCauseWithProtErr
. . . . . laterNonCriticalExtensions
- Constraint:
car_RRC_ConnRelCmplUM
- BinaryMessage:
30 0e 02 01 ff 02 01 01 05 00 d6 d7 48 1c 8c 40

- No.: 2933
- Timestamp: 17:29:56:456_1
- RFN: 79522
- Chip: 30720
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ConnRel:lt_Send_RRC_ConnectionRelease LINE 4
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2936
- Timestamp: 17:29:56:457_0
- RFN: 79522
- Chip: 33024
- Event: Start Timer
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 1
- Message Structure:
no details available
- Constraint:
t_Dly (5000 Ms)
- BinaryMessage:

- No.: 2940
- Timestamp: 17:29:56:616_0
- RFN: 79538
- Chip: 28672
- Event: Receive
- PCO: UM
- Message: RLC_UM_DATA_IND
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 4
- Message Structure:
RLC_UM_DATA_IND
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 1
. IntegrityResult
. uM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00011100010101000111110101101001"
. . . . (IntegerType)rrc_MessageSequenceNumber[4] = 2
. . . UL_DCCH_MessageType
. . . . RRCConnectionReleaseComplete
. . . . . (IntegerType)rrc_TransactionIdentifier[2] = 0
. . . . . FailureCauseWithProtErr
. . . . . laterNonCriticalExtensions
- Constraint:
car_RRC_ConnRelCmplUM
- BinaryMessage:
30 0e 02 01 ff 02 01 01 05 00 8e 2a 3e b4 94 40

- No.: 2941
- Timestamp: 17:29:56:616_1
- RFN: 79538
- Chip: 30208
- Event: Cancel Timer
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 4
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 2942
- Timestamp: 17:29:56:616_2
- RFN: 79538
- Chip: 30464
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 4
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2948
- Timestamp: 17:29:56:618_0
- RFN: 79538
- Chip: 35328
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 1
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 01 0a 01 00 05 00

- No.: 2952
- Timestamp: 17:29:56:624_0
- RFN: 79539
- Chip: 21248
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 2955
- Timestamp: 17:29:56:625_0
- RFN: 79539
- Chip: 24576
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 2
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 02 0a 01 00 05 00

- No.: 2959
- Timestamp: 17:29:56:628_0
- RFN: 79539
- Chip: 36608
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 2962
- Timestamp: 17:29:56:629_0
- RFN: 79540
- Chip: 1280
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 3
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 03 0a 01 00 05 00

- No.: 2966
- Timestamp: 17:29:56:635_0
- RFN: 79540
- Chip: 23808
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 3
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 2969
- Timestamp: 17:29:56:635_3
- RFN: 79540
- Chip: 26880
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 4
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 04 0a 01 00 05 00

- No.: 2973
- Timestamp: 17:29:56:642_0
- RFN: 79541
- Chip: 13824
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 4
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 2976
- Timestamp: 17:29:56:644_0
- RFN: 79541
- Chip: 20480
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 1
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 136
. . . . . UL_RLC_Mode
. . . . . . UL_UM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (NoExplicitDiscard)timerBasedNoExplicit[0] = 9
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 1
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 1
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_UM_Info
- BinaryMessage:
30 22 02 01 ff 02 01 01 0a 01 00 30 17 30 0d 05 00 30 09 02 02 00 88 30 03 0a 01 09 30 06 02 01 01 02 01 01

- No.: 2980
- Timestamp: 17:29:56:649_0
- RFN: 79542
- Chip: 512
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 2981
- Timestamp: 17:29:56:650_0
- RFN: 79542
- Chip: 6912
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 3
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 2
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 2
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 2
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 02 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 13 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 02 02 01 02

- No.: 2985
- Timestamp: 17:29:56:658_0
- RFN: 79542
- Chip: 36096
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 4
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 2986
- Timestamp: 17:29:56:659_0
- RFN: 79543
- Chip: 4096
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 5
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 3
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 3
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 3
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 03 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 13 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 03 02 01 03

- No.: 2990
- Timestamp: 17:29:56:668_0
- RFN: 79543
- Chip: 37632
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 6
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 3
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 2991
- Timestamp: 17:29:56:670_0
- RFN: 79544
- Chip: 5888
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 7
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 4
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 4
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 4
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 04 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 13 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 04 02 01 04

- No.: 2995
- Timestamp: 17:29:56:678_0
- RFN: 79544
- Chip: 38144
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 8
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 4
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 3020
- Timestamp: 17:29:56:681_7
- RFN: 79545
- Chip: 11520
- Event: Start Timer
- Source: ts_NAS_Delay LINE 1
- Message Structure:
no details available
- Constraint:
t_Dly (5000 Ms)
- BinaryMessage:

- No.: 3027
- Timestamp: 17:30:01:674_0
- RFN: 80044
- Chip: 22528
- Event: Timeout
- Source: ts_NAS_Delay LINE 2
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 3034
- Timestamp: 17:30:01:675_1
- RFN: 80044
- Chip: 27648
- Event: Send
- PCO: Ut
- Message: MMI_CmdReq
- Source: ts_MMI_UE_SwitchOff LINE 2
- Message Structure:
MMI_CmdReq
. (IA5StringType)cmd[-1] = "Please switch off the UE"
- Constraint:
ca_MMI_CmdReq
- BinaryMessage:
50 6c 65 61 73 65 20 73 77 69 74 63 68 20 6f 66 66 20 20 74 68 65 20 55 45

- No.: 3038
- Timestamp: 17:30:05:847_0
- RFN: 80461
- Chip: 37888
- Event: Receive
- PCO: Ut
- Message: MMI_CmdCnf
- Source: ts_MMI_UE_SwitchOff LINE 3
- Message Structure:
MMI_CmdCnf
. (BooleanType)result = TRUE
. (IA5StringType)resultString[6] = " OK "
- Constraint:
ca_MMI_CmdCnf
- BinaryMessage:
80 0d 0a 4f 4b 0d 0a

- No.: 3057
- Timestamp: 17:30:05:850_0
- RFN: 80462
- Chip: 8960
- Event: Receive
- PCO: CPHY
- Message: CPHY_Out_of_Sync_IND
- Source: RRC_DefConnEst LINE 7
- Message Structure:
CPHY_Out_of_Sync_IND
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 20
- Constraint:
ca_OutOfSyncInd
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 3058
- Timestamp: 17:30:05:850_1
- RFN: 80462
- Chip: 9728
- Event: Cancel Timer
- Source: RRC_DefConnEst LINE 7
- Message Structure:
no details available
- Constraint:
t_T312
- BinaryMessage:

- No.: 3059
- Timestamp: 17:30:05:850_2
- RFN: 80462
- Chip: 10496
- Event: Default
- Source: RRC_DefConnEst LINE 0
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3060
- Timestamp: 17:30:05:850_3
- RFN: 80462
- Chip: 10752
- Event: Default
- Source: ts_RRC_ConnEst:lt_RcvConnReq LINE 4
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3065
- Timestamp: 17:30:06:927_0
- RFN: 80569
- Chip: 35840
- Event: Receive
- PCO: TM
- Message: RLC_TR_DATA_IND
- Source: ts_RRC_ConnEst:lt_RcvConnReq LINE 4
- Message Structure:
RLC_TR_DATA_IND
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 0
. tM_message
. . UL_CCCH_Message
. . . IntegrityCheckInfo
. . . UL_CCCH_MessageType
. . . . RRCConnectionRequest
. . . . . InitialUE_Identity
. . . . . . TMSI_and_LAI_GSM_MAP
. . . . . . . (BitStringType)tmsi[32] = "00010010001101000101011001111000"
. . . . . . . LAI
. . . . . . . . PLMN_Identity
. . . . . . . . . MCC
. . . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . . (IntegerType)_elem[4] = 1
. . . . . . . . . MNC
. . . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . . (IntegerType)_elem[4] = 1
. . . . . . . . (BitStringType)lac[16] = '0000000000000001'B
. . . . . (EstablishmentCause)establishmentCause[5] = 13
. . . . . (ProtocolErrorIndicator)protocolErrorIndicator[1] = 0
. . . . . MeasuredResultsOnRACH
. . . . . v3d0NonCriticalExtensions
- Constraint:
car_RRC_ConnReq
- BinaryMessage:
30 11 02 01 00 02 01 00 21 12 34 56 78 00 10 08 00 0b 40

- No.: 3069
- Timestamp: 17:30:06:937_0
- RFN: 80570
- Chip: 35328
- Event: Send
- PCO: UM
- Message: RLC_UM_DATA_REQ
- Source: ts_RRC_ConnEst:lt_Send_ConnSetUp LINE 22
- Message Structure:
RLC_UM_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 0
. uM_message
. . DL_CCCH_Message
. . . IntegrityCheckInfo
. . . DL_CCCH_MessageType
. . . . RRCConnectionSetup
. . . . . r3
. . . . . . RRCConnectionSetup_r3_IEs
. . . . . . . InitialUE_Identity
. . . . . . . . TMSI_and_LAI_GSM_MAP
. . . . . . . . . (BitStringType)tmsi[32] = "00010010001101000101011001111000"
. . . . . . . . . LAI
. . . . . . . . . . PLMN_Identity
. . . . . . . . . . . MCC
. . . . . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . . . . (IntegerType)_elem[4] = 1
. . . . . . . . . . . MNC
. . . . . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . . . . (IntegerType)_elem[4] = 1
. . . . . . . . . . (BitStringType)lac[16] = '0000000000000001'B
. . . . . . . (IntegerType)rrc_TransactionIdentifier[-1] = 0
. . . . . . . (IntegerType)activationTime[-1] = -
. . . . . . . U_RNTI
. . . . . . . . (BitStringType)srnc_Identity[12] = "000000000001"
. . . . . . . . (BitStringType)s_RNTI[20] = "00000000000000000001"
. . . . . . . (BitStringType)new_c_RNTI[16] = -
. . . . . . . (RRC_StateIndicator)rrc_StateIndicator[0] = 0
. . . . . . . (IntegerType)utran_DRX_CycleLengthCoeff[-1] = 9
. . . . . . . CapabilityUpdateRequirement
. . . . . . . . (BooleanType)ue_RadioCapabilityFDDUpdateRequirement = TRUE
. . . . . . . . (BooleanType)ue_RadioCapabilityTDDUpdateRequirement = FALSE
. . . . . . . . SystemSpecificCapUpdateReqList
. . . . . . . . . (SystemSpecificCapUpdateReq)_elem[0] = 0
. . . . . . . SRB_InformationSetupList2
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity[-1] = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_UM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 1
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex[-1] = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 1
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity[-1] = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 2
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 2
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 2
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 2
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex[-1] = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 2
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 2
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity[-1] = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 3
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 3
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 3
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 3
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex[-1] = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 3
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 3
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity[-1] = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 4
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 4
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 4
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 4
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex[-1] = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 4
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 4
. . . . . . . UL_CommonTransChInfo
. . . . . . . . TFC_Subset
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . TFCS
. . . . . . . . . . . ExplicitTFCS_Configuration
. . . . . . . . . . . . TFCS_ReconfAdd
. . . . . . . . . . . . . ctfcSize
. . . . . . . . . . . . . . ctfc2Bit
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . . . . . . . (IntegerType)ctfc2[-1] = 0
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . . . . . . . (IntegerType)ctfc2[-1] = 1
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC[-1] = 11
. . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaD[-1] = 15
. . . . . . . . . . . . . . . . . . . (IntegerType)referenceTFC_ID[-1] = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . UL_AddReconfTransChInfoList
. . . . . . . . UL_AddReconfTransChInformation
. . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType[0] = 0
. . . . . . . . . (IntegerType)transportChannelIdentity[-1] = 5
. . . . . . . . . TransportFormatSet
. . . . . . . . . . DedicatedTransChTFS
. . . . . . . . . . . tti
. . . . . . . . . . . . DedicatedDynamicTF_InfoList
. . . . . . . . . . . . . DedicatedDynamicTF_Info
. . . . . . . . . . . . . . rlc_Size
. . . . . . . . . . . . . . . BitModeRLC_SizeInfo
. . . . . . . . . . . . . . . . sizeType2
. . . . . . . . . . . . . . . . . (IntegerType)part1[-1] = 2
. . . . . . . . . . . . . . . . . (IntegerType)part2[-1] = -
. . . . . . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . LogicalChannelList
. . . . . . . . . . . SemistaticTF_Information
. . . . . . . . . . . . ChannelCodingType
. . . . . . . . . . . . . (CodingRate)convolutional[0] = 1
. . . . . . . . . . . . (IntegerType)rateMatchingAttribute[-1] = 192
. . . . . . . . . . . . (CRC_Size)crc_Size[0] = 3
. . . . . . . DL_CommonTransChInfo
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . dl_Parameters
. . . . . . . DL_AddReconfTransChInfoList
. . . . . . . . DL_AddReconfTransChInformation
. . . . . . . . . (DL_TrCH_Type)dl_TransportChannelType[0] = 0
. . . . . . . . . (IntegerType)dl_transportChannelIdentity[-1] = 10
. . . . . . . . . tfs_SignallingMode
. . . . . . . . . . UL_TransportChannelIdentity
. . . . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType[0] = 0
. . . . . . . . . . . (IntegerType)ul_TransportChannelIdentity[-1] = 5
. . . . . . . . . QualityTarget
. . . . . . . . . . (IntegerType)bler_QualityValue[-1] = -20
. . . . . . . . . TM_SignallingInfo
. . . . . . . FrequencyInfo
. . . . . . . (IntegerType)maxAllowedUL_TX_Power[-1] = -
. . . . . . . UL_ChannelRequirement
. . . . . . . . UL_DPCH_Info
. . . . . . . . . UL_DPCH_PowerControlInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (IntegerType)dpcch_PowerOffset[-1] = -40
. . . . . . . . . . . (IntegerType)pc_Preamble[-1] = 1
. . . . . . . . . . . (IntegerType)sRB_delay[-1] = 7
. . . . . . . . . . . PowerControlAlgorithm
. . . . . . . . . . . . (IntegerType)algorithm1[-1] = 1
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (ScramblingCodeType)scramblingCodeType[0] = 1
. . . . . . . . . . . (IntegerType)scramblingCode[-1] = 0
. . . . . . . . . . . (IntegerType)numberOfDPDCH[-1] = -
. . . . . . . . . . . (SpreadingFactor)spreadingFactor[0] = 4
. . . . . . . . . . . (BooleanType)tfci_Existence = TRUE
. . . . . . . . . . . (IntegerType)numberOfFBI_Bits[-1] = -
. . . . . . . . . . . (PuncturingLimit)puncturingLimit[0] = 15
. . . . . . . DL_CommonInformation
. . . . . . . . DL_DPCH_InfoCommon
. . . . . . . . . cfnHandling
. . . . . . . . . . initialise
. . . . . . . . . . . (IntegerType)cfntargetsfnframeoffset[-1] = -
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . DL_DPCH_PowerControlInfo
. . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . (DPC_Mode)dpc_Mode[0] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPilot_pdpdch[-1] = 0
. . . . . . . . . . . Dl_rate_matching_restriction
. . . . . . . . . . . SF512_AndPilot
. . . . . . . . . . . . (PilotBits128)sfd128[0] = 0
. . . . . . . . . . . (PositionFixedOrFlexible)positionFixedOrFlexible[0] = 0
. . . . . . . . . . . (BooleanType)tfci_Existence = FALSE
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . (IntegerType)defaultDPCH_OffsetValue[-1] = 459
. . . . . . . . . . DPCH_CompressedModeInfo
. . . . . . . . . . (TX_DiversityMode)tx_DiversityMode[0] = 0
. . . . . . . . . . SSDT_Information
. . . . . . . DL_InformationPerRL_List
. . . . . . . . DL_InformationPerRL
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . PrimaryCPICH_Info
. . . . . . . . . . . . (IntegerType)primaryScramblingCode[-1] = 100
. . . . . . . . . . . PDSCH_SHO_DCH_Info
. . . . . . . . . . . PDSCH_CodeMapping
. . . . . . . . . DL_DPCH_InfoPerRL
. . . . . . . . . . fdd
. . . . . . . . . . . (PCPICH_UsageForChannelEst)pCPICH_UsageForChannelEst[0] = 0
. . . . . . . . . . . (IntegerType)dpch_FrameOffset[-1] = 18
. . . . . . . . . . . SecondaryCPICH_Info
. . . . . . . . . . . DL_ChannelisationCodeList
. . . . . . . . . . . . DL_ChannelisationCode
. . . . . . . . . . . . . (IntegerType)secondaryScramblingCode[-1] = 1
. . . . . . . . . . . . . SF512_AndCodeNumber
. . . . . . . . . . . . . . (IntegerType)sf128[-1] = 0
. . . . . . . . . . . . . (ScramblingCodeChange)scramblingCodeChange[0] = 1
. . . . . . . . . . . (IntegerType)tpc_CombinationIndex[-1] = 0
. . . . . . . . . . . (SSDT_CellIdentity)ssdt_CellIdentity[0] = -
. . . . . . . . . . . (ClosedLoopTimingAdjMode)closedLoopTimingAdjMode[0] = -
. . . . . . . . . SCCPCH_InfoForFACH
. . . . . . laterNonCriticalExtensions
. (BooleanType)specialLI = TRUE
- Constraint:
cas_RRC_ConnSetup
- BinaryMessage:
30 78 02 01 00 02 01 00 30 e7 22 46 8a cf 00 02 01 00 01 00 04 00 00 4d 82 69 3a 10 10 89 0d 42 00 02 81 9e 8e 46 c9 a6 7c 9c 4e 74 20 a5 12 3a 8c 00 15 13 3d 1c 8d 93 4c f9 38 9c e8 42 52 24 b5 28 00 4a 46 7a 39 1b 26 99 f2 71 39 d0 86 b4 49 ea 70 00 d4 c8 00 06 25 2b f0 02 00 08 82 23 bf 66 08 98 95 a5 47 a2 00 00 01 3f 90 0a 14 e5 82 06 40 09 0c 28 08 01 01 ff

- No.: 3090
- Timestamp: 17:30:06:959_4
- RFN: 80573
- Chip: 5888
- Event: Start Timer
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 3
- Message Structure:
no details available
- Constraint:
t_WaitMS (13500 Ms)
- BinaryMessage:

- No.: 3097
- Timestamp: 17:30:07:145_0
- RFN: 80591
- Chip: 29440
- Event: Receive
- PCO: CPHY
- Message: CPHY_Sync_IND
- Source: RRC_DefConnEst LINE 5
- Message Structure:
CPHY_Sync_IND
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 20
- Constraint:
ca_SyncInd
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 3098
- Timestamp: 17:30:07:145_1
- RFN: 80591
- Chip: 30208
- Event: Cancel Timer
- Source: RRC_DefConnEst LINE 5
- Message Structure:
no details available
- Constraint:
t_T312
- BinaryMessage:

- No.: 3099
- Timestamp: 17:30:07:145_2
- RFN: 80591
- Chip: 30976
- Event: Default
- Source: RRC_DefConnEst LINE 0
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3100
- Timestamp: 17:30:07:145_3
- RFN: 80591
- Chip: 31232
- Event: Default
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3107
- Timestamp: 17:30:07:247_0
- RFN: 80601
- Chip: 36096
- Event: Receive
- PCO: AM
- Message: RLC_AM_DATA_IND
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
RLC_AM_DATA_IND
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 2
. IntegrityResult
. . (IntegrityStatus)integrityUsed[0] = 4294967296
. aM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . UL_DCCH_MessageType
. . . . RRCConnectionSetupComplete
. . . . . (IntegerType)rrc_TransactionIdentifier[2] = 0
. . . . . STARTList
. . . . . . STARTSingle
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity[1] = 1
. . . . . . . (BitStringType)start_Value[20] = "00000000000000000010"
. . . . . . STARTSingle
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity[1] = 0
. . . . . . . (BitStringType)start_Value[20] = "00000000000000000010"
. . . . . UE_RadioAccessCapability
. . . . . . (AccessStratumReleaseIndicator)accessStratumReleaseIndicator[0] = 0
. . . . . . PDCP_Capability
. . . . . . . (BooleanType)losslessSRNS_RelocationSupport = FALSE
. . . . . . . supportForRfc2507
. . . . . . . . (MaxHcContextSpace)supported[3] = 4
. . . . . . RLC_Capability
. . . . . . . (TotalRLC_AM_BufferSize)totalRLC_AM_BufferSize[3] = 2
. . . . . . . (MaximumRLC_WindowSize)maximumRLC_WindowSize[1] = 0
. . . . . . . (MaximumAM_EntityNumberRLC_Cap)maximumAM_EntityNumber[3] = 3
. . . . . . TransportChannelCapability
. . . . . . . DL_TransChCapability
. . . . . . . . (MaxNoBits)maxNoBitsReceived[4] = 7
. . . . . . . . (MaxNoBits)maxConvCodeBitsReceived[4] = 1
. . . . . . . . TurboSupport
. . . . . . . . . (MaxNoBits)supported[4] = 7
. . . . . . . . (MaxSimultaneousTransChsDL)maxSimultaneousTransChs[2] = 1
. . . . . . . . (IntegerType)maxSimultaneousCCTrCH_Count[3] = 1
. . . . . . . . (MaxTransportBlocksDL)maxReceivedTransportBlocks[4] = 3
. . . . . . . . (MaxNumberOfTFC_DL)maxNumberOfTFC[4] = 5
. . . . . . . . (MaxNumberOfTF)maxNumberOfTF[3] = 1
. . . . . . . UL_TransChCapability
. . . . . . . . (MaxNoBits)maxNoBitsTransmitted[4] = 3
. . . . . . . . (MaxNoBits)maxConvCodeBitsTransmitted[4] = 1
. . . . . . . . TurboSupport
. . . . . . . . . (MaxNoBits)supported[4] = 3
. . . . . . . . (MaxSimultaneousTransChsUL)maxSimultaneousTransChs[3] = 2
. . . . . . . . modeSpecificInfo
. . . . . . . . (MaxTransportBlocksUL)maxTransmittedBlocks[4] = 4
. . . . . . . . (MaxNumberOfTFC_UL)maxNumberOfTFC[4] = 5
. . . . . . . . (MaxNumberOfTF)maxNumberOfTF[3] = 0
. . . . . . RF_Capability
. . . . . . . fddRF_Capability
. . . . . . . . (IntegerType)ue_PowerClass[2] = 4
. . . . . . . . (TxRxFrequencySeparation)txRxFrequencySeparation[2] = 0
. . . . . . . tddRF_Capability
. . . . . . PhysicalChannelCapability
. . . . . . . fddPhysChCapability
. . . . . . . . DL_PhysChCapabilityFDD
. . . . . . . . . (IntegerType)maxNoDPCH_PDSCH_Codes[3] = 1
. . . . . . . . . (MaxNoPhysChBitsReceived)maxNoPhysChBitsReceived[4] = 6
. . . . . . . . . (BooleanType)supportForSF_512 = FALSE
. . . . . . . . . (BooleanType)supportOfPDSCH = FALSE
. . . . . . . . . SimultaneousSCCPCH_DPCH_Reception
. . . . . . . . UL_PhysChCapabilityFDD
. . . . . . . . . (MaxNoDPDCH_BitsTransmitted)maxNoDPDCH_BitsTransmitted[4] = 3
. . . . . . . . . (BooleanType)supportOfPCPCH = FALSE
. . . . . . . tddPhysChCapability
. . . . . . UE_MultiModeRAT_Capability
. . . . . . . MultiRAT_Capability
. . . . . . . . (BooleanType)supportOfGSM = FALSE
. . . . . . . . (BooleanType)supportOfMulticarrier = FALSE
. . . . . . . (MultiModeCapability)multiModeCapability[2] = 1
. . . . . . SecurityCapability
. . . . . . . (BitStringType)cipheringAlgorithmCap[16] = '0000000000000011'B
. . . . . . . (BitStringType)integrityProtectionAlgorithmCap[16] = '0000000000000010'B
. . . . . . UE_Positioning_Capability
. . . . . . . (BooleanType)standaloneLocMethodsSupported = FALSE
. . . . . . . (BooleanType)ue_BasedOTDOA_Supported = FALSE
. . . . . . . (NetworkAssistedGPS_Supported)networkAssistedGPS_Supported[2] = 3
. . . . . . . (BooleanType)supportForUE_GPS_TimingOfCellFrames = FALSE
. . . . . . . (BooleanType)supportForIPDL = FALSE
. . . . . . MeasurementCapability
. . . . . . . CompressedModeMeasCapability
. . . . . . . . (BooleanType)fdd_Measurements = TRUE
. . . . . . . . (BooleanType)tdd_Measurements = -
. . . . . . . . GSM_Measurements
. . . . . . . . . (BooleanType)gsm900 = TRUE
. . . . . . . . . (BooleanType)dcs1800 = TRUE
. . . . . . . . . (BooleanType)gsm1900 = TRUE
. . . . . . . . (BooleanType)multiCarrierMeasurements = FALSE
. . . . . . . CompressedModeMeasCapability
. . . . . . . . (BooleanType)fdd_Measurements = TRUE
. . . . . . . . (BooleanType)tdd_Measurements = -
. . . . . . . . GSM_Measurements
. . . . . . . . . (BooleanType)gsm900 = TRUE
. . . . . . . . . (BooleanType)dcs1800 = TRUE
. . . . . . . . . (BooleanType)gsm1900 = TRUE
. . . . . . . . (BooleanType)multiCarrierMeasurements = FALSE
. . . . . v370NonCriticalExtensions
- Constraint:
car_RRC_ConnSetupCmpl
- BinaryMessage:
30 27 02 01 ff 02 01 02 0a 05 01 00 00 00 00 4a 0c 00 00 80 00 05 62 37 1b a0 d4 98 cd 11 45 90 60 61 00 03 00 02 31 f9 f8

- No.: 3108
- Timestamp: 17:30:07:249_0
- RFN: 80602
- Chip: 4608
- Event: Cancel Timer
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
t_WaitMS
- BinaryMessage:

- No.: 3109
- Timestamp: 17:30:07:249_1
- RFN: 80602
- Chip: 4864
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3127
- Timestamp: 17:30:07:266_0
- RFN: 80603
- Chip: 30976
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_MM_IMSI_Detach:lt_IMSI_Detach LINE 2
- Message Structure:
RRC_DataInd
. (IntegerType)cellId[0] = -1
. (SS_RB_Identity)rB_Id[0] = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain[0] = 0
. (START_Value)start[20] = '00000000000000000010'B
. IMSIDETACHINDICATION
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)mMProtocolDiscriminator[4] = '0101'B
. . (MsgType)msgType[8] = '00000001'B
. . MS_Clsmk1
. . . (B1)spare1[1] = '0'B
. . . (B2)revLvl[2] = '10'B
. . . (B1)eSIND[1] = '0'B
. . . (B1)a5_1[1] = '1'B
. . . (B3)rFPwrCap[3] = '111'B
. . MS_Identity_lv
. . . (Length)iel[1] = '05'O
. . . (B4)iDigit1[4] = '1111'B
. . . (B1)oddEvenInd[1] = '0'B
. . . (B3)typeOfId[3] = '100'B
. . . (OctetStringType)otherDigits[4] = '12345678'O
- Constraint:
car_InitDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 00 03 04 04 00 00 20 05 01 4f 05 f4 12 34 56 78

- No.: 3128
- Timestamp: 17:30:07:266_1
- RFN: 80603
- Chip: 32256
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_MM_IMSI_Detach:lt_IMSI_Detach LINE 2
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3140
- Timestamp: 17:30:07:268_0
- RFN: 80603
- Chip: 38144
- Event: Start Timer
- Source: ts_RRC_Delay LINE 1
- Message Structure:
no details available
- Constraint:
t_Dly (1000 Ms)
- BinaryMessage:

- No.: 3144
- Timestamp: 17:30:08:254_0
- RFN: 80702
- Chip: 24576
- Event: Timeout
- Source: ts_RRC_Delay LINE 2
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 3149
- Timestamp: 17:30:08:255_0
- RFN: 80702
- Chip: 29184
- Event: Send
- PCO: UM
- Message: RLC_UM_DATA_REQ
- Source: ts_RRC_ConnRel:lt_Send_RRC_ConnectionRelease LINE 3
- Message Structure:
RLC_UM_DATA_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 1
. uM_message
. . DL_DCCH_Message
. . . IntegrityCheckInfo
. . . DL_DCCH_MessageType
. . . . RRCConnectionRelease
. . . . . r3
. . . . . . RRCConnectionRelease_r3_IEs
. . . . . . . (IntegerType)rrc_TransactionIdentifier[-1] = 0
. . . . . . . (IntegerType)n_308[-1] = 1
. . . . . . . (ReleaseCause)releaseCause[0] = 0
. . . . . . . Rplmn_Information
. . . . . . laterNonCriticalExtensions
. (BooleanType)specialLI = FALSE
- Constraint:
cas_RRC_ConnRelDCCH
- BinaryMessage:
30 0c 02 01 ff 02 01 01 3c 80 00 01 01 00

- No.: 3153
- Timestamp: 17:30:08:374_0
- RFN: 80714
- Chip: 28416
- Event: Receive
- PCO: UM
- Message: RLC_UM_DATA_IND
- Source: ts_RRC_ConnRel:lt_Send_RRC_ConnectionRelease LINE 4
- Message Structure:
RLC_UM_DATA_IND
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 1
. IntegrityResult
. uM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . UL_DCCH_MessageType
. . . . RRCConnectionReleaseComplete
. . . . . (IntegerType)rrc_TransactionIdentifier[2] = 0
. . . . . FailureCauseWithProtErr
. . . . . laterNonCriticalExtensions
- Constraint:
car_RRC_ConnRelCmplUM
- BinaryMessage:
30 0a 02 01 ff 02 01 01 05 00 44 00

- No.: 3154
- Timestamp: 17:30:08:375_0
- RFN: 80714
- Chip: 29696
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ConnRel:lt_Send_RRC_ConnectionRelease LINE 4
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3157
- Timestamp: 17:30:08:375_3
- RFN: 80714
- Chip: 31488
- Event: Start Timer
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 1
- Message Structure:
no details available
- Constraint:
t_Dly (5000 Ms)
- BinaryMessage:

- No.: 3161
- Timestamp: 17:30:08:535_0
- RFN: 80730
- Chip: 28672
- Event: Receive
- PCO: UM
- Message: RLC_UM_DATA_IND
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 4
- Message Structure:
RLC_UM_DATA_IND
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 1
. IntegrityResult
. uM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . UL_DCCH_MessageType
. . . . RRCConnectionReleaseComplete
. . . . . (IntegerType)rrc_TransactionIdentifier[2] = 0
. . . . . FailureCauseWithProtErr
. . . . . laterNonCriticalExtensions
- Constraint:
car_RRC_ConnRelCmplUM
- BinaryMessage:
30 08 02 01 ff 02 01 01 44 00

- No.: 3162
- Timestamp: 17:30:08:535_1
- RFN: 80730
- Chip: 29952
- Event: Cancel Timer
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 4
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 3163
- Timestamp: 17:30:08:535_2
- RFN: 80730
- Chip: 30208
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 4
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3169
- Timestamp: 17:30:08:537_0
- RFN: 80730
- Chip: 35328
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 1
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 01 0a 01 00 05 00

- No.: 3173
- Timestamp: 17:30:08:542_0
- RFN: 80731
- Chip: 19200
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 3176
- Timestamp: 17:30:08:543_2
- RFN: 80731
- Chip: 22528
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 2
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 02 0a 01 00 05 00

- No.: 3180
- Timestamp: 17:30:08:547_0
- RFN: 80731
- Chip: 35584
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 3183
- Timestamp: 17:30:08:548_0
- RFN: 80732
- Chip: 512
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 3
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 03 0a 01 00 05 00

- No.: 3187
- Timestamp: 17:30:08:554_0
- RFN: 80732
- Chip: 25344
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 3
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 3190
- Timestamp: 17:30:08:555_0
- RFN: 80732
- Chip: 28672
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 4
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 04 0a 01 00 05 00

- No.: 3194
- Timestamp: 17:30:08:562_0
- RFN: 80733
- Chip: 17664
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 4
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 3197
- Timestamp: 17:30:08:564_0
- RFN: 80733
- Chip: 24064
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 1
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 136
. . . . . UL_RLC_Mode
. . . . . . UL_UM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (NoExplicitDiscard)timerBasedNoExplicit[0] = 9
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 1
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 1
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_UM_Info
- BinaryMessage:
30 22 02 01 ff 02 01 01 0a 01 00 30 17 30 0d 05 00 30 09 02 02 00 88 30 03 0a 01 09 30 06 02 01 01 02 01 01

- No.: 3201
- Timestamp: 17:30:08:568_0
- RFN: 80734
- Chip: 1280
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 3202
- Timestamp: 17:30:08:569_0
- RFN: 80734
- Chip: 7424
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 3
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 2
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 2
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 2
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 02 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 13 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 02 02 01 02

- No.: 3206
- Timestamp: 17:30:08:578_0
- RFN: 80735
- Chip: 1024
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 4
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 3207
- Timestamp: 17:30:08:579_0
- RFN: 80735
- Chip: 7680
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 5
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 3
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 3
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 3
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 03 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 13 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 03 02 01 03

- No.: 3211
- Timestamp: 17:30:08:588_0
- RFN: 80736
- Chip: 1536
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 6
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 3
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 3212
- Timestamp: 17:30:08:589_0
- RFN: 80736
- Chip: 8192
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 7
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 4
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 4
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 4
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 04 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 13 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 04 02 01 04

- No.: 3216
- Timestamp: 17:30:08:598_0
- RFN: 80737
- Chip: 2048
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 8
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 4
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 3239
- Timestamp: 17:30:08:601_1
- RFN: 80737
- Chip: 13056
- Event: Start Timer
- Source: ts_RRC_ConnRejectGMM_Detach LINE 1
- Message Structure:
no details available
- Constraint:
t_Dly (2000 Ms)
- BinaryMessage:

- No.: 3244
- Timestamp: 17:30:08:674_0
- RFN: 80744
- Chip: 25856
- Event: Receive
- PCO: CPHY
- Message: CPHY_Out_of_Sync_IND
- Source: RRC_DefConnEst LINE 7
- Message Structure:
CPHY_Out_of_Sync_IND
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 20
- Constraint:
ca_OutOfSyncInd
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 3245
- Timestamp: 17:30:08:674_1
- RFN: 80744
- Chip: 26624
- Event: Cancel Timer
- Source: RRC_DefConnEst LINE 7
- Message Structure:
no details available
- Constraint:
t_T312
- BinaryMessage:

- No.: 3246
- Timestamp: 17:30:08:674_2
- RFN: 80744
- Chip: 27136
- Event: Default
- Source: RRC_DefConnEst LINE 0
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3247
- Timestamp: 17:30:08:674_3
- RFN: 80744
- Chip: 27648
- Event: Default
- Source: ts_RRC_ConnRejectGMM_Detach LINE 4
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3252
- Timestamp: 17:30:10:600_0
- RFN: 80937
- Chip: 11776
- Event: Timeout
- Source: ts_RRC_ConnRejectGMM_Detach LINE 4
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 3288
- Timestamp: 17:30:10:605_0
- RFN: 80937
- Chip: 29952
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 1
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 01 0a 01 00 05 00

- No.: 3292
- Timestamp: 17:30:10:607_0
- RFN: 80938
- Chip: 2816
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 3295
- Timestamp: 17:30:10:608_2
- RFN: 80938
- Chip: 5888
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 2
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 02 0a 01 00 05 00

- No.: 3299
- Timestamp: 17:30:10:613_0
- RFN: 80938
- Chip: 25344
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 3302
- Timestamp: 17:30:10:614_1
- RFN: 80938
- Chip: 28928
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 3
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 03 0a 01 00 05 00

- No.: 3306
- Timestamp: 17:30:10:617_0
- RFN: 80939
- Chip: 2304
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 3
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 3309
- Timestamp: 17:30:10:618_1
- RFN: 80939
- Chip: 5376
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 4
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 04 0a 01 00 05 00

- No.: 3313
- Timestamp: 17:30:10:623_0
- RFN: 80939
- Chip: 24576
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 4
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 3317
- Timestamp: 17:30:10:624_0
- RFN: 80939
- Chip: 29184
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_CMAC_Rel LINE 1
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 26
. (RatType)ratType[0] = 0
. configMessage
- Constraint:
cas_MAC_Rel
- BinaryMessage:
30 0b 02 01 ff 02 01 1a 0a 01 00 05 00

- No.: 3321
- Timestamp: 17:30:10:626_0
- RFN: 80939
- Chip: 37120
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_CMAC_Rel LINE 2
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 26
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 1a

- No.: 3324
- Timestamp: 17:30:10:627_1
- RFN: 80940
- Chip: 2304
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_CMAC_Rel LINE 1
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 20
. (RatType)ratType[0] = 0
. configMessage
- Constraint:
cas_MAC_Rel
- BinaryMessage:
30 0b 02 01 ff 02 01 14 0a 01 00 05 00

- No.: 3328
- Timestamp: 17:30:10:631_0
- RFN: 80940
- Chip: 15360
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_CMAC_Rel LINE 2
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 20
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 14

- No.: 3331
- Timestamp: 17:30:10:631_3
- RFN: 80940
- Chip: 17920
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Release_REQ
- Source: ts_CPHY_TrChRelDCH_NoSHO LINE 1
- Message Structure:
CPHY_TrCH_Release_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 26
. TrChConfigType
. . (TrChConfigType_list_0)dch[0] = 0
- Constraint:
ca_PHY_RelReqDCH_NoSHO
- BinaryMessage:
30 09 02 01 00 02 01 1a 0a 01 00

- No.: 3335
- Timestamp: 17:30:10:636_0
- RFN: 80940
- Chip: 36608
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Release_CNF
- Source: ts_CPHY_TrChRelDCH_NoSHO LINE 2
- Message Structure:
CPHY_TrCH_Release_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 26
- Constraint:
ca_PHY_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 1a

- No.: 3338
- Timestamp: 17:30:10:637_0
- RFN: 80941
- Chip: 1024
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Release_REQ
- Source: ts_CPHY_TrChRelDCH_NoSHO LINE 1
- Message Structure:
CPHY_TrCH_Release_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 20
. TrChConfigType
. . (TrChConfigType_list_0)dch[0] = 0
- Constraint:
ca_PHY_RelReqDCH_NoSHO
- BinaryMessage:
30 09 02 01 00 02 01 14 0a 01 00

- No.: 3342
- Timestamp: 17:30:10:664_0
- RFN: 80943
- Chip: 25600
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Release_CNF
- Source: ts_CPHY_TrChRelDCH_NoSHO LINE 2
- Message Structure:
CPHY_TrCH_Release_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 20
- Constraint:
ca_PHY_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 3345
- Timestamp: 17:30:10:665_1
- RFN: 80943
- Chip: 28416
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 26
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 1a

- No.: 3349
- Timestamp: 17:30:10:672_0
- RFN: 80944
- Chip: 17152
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 26
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 1a

- No.: 3352
- Timestamp: 17:30:10:673_0
- RFN: 80944
- Chip: 19712
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 20
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 3356
- Timestamp: 17:30:10:697_0
- RFN: 80946
- Chip: 37888
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 20
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 3361
- Timestamp: 17:30:10:698_3
- RFN: 80947
- Chip: 3840
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 0
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 00 02 01 00 0a 01 00 05 00

- No.: 3365
- Timestamp: 17:30:10:702_0
- RFN: 80947
- Chip: 16896
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 0
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 00

- No.: 3368
- Timestamp: 17:30:10:703_0
- RFN: 80947
- Chip: 20224
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_CMAC_Rel LINE 1
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 8
. (RatType)ratType[0] = 0
. configMessage
- Constraint:
cas_MAC_Rel
- BinaryMessage:
30 0b 02 01 00 02 01 08 0a 01 00 05 00

- No.: 3372
- Timestamp: 17:30:10:705_0
- RFN: 80947
- Chip: 30464
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_CMAC_Rel LINE 2
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 8
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 08

- No.: 3375
- Timestamp: 17:30:10:706_1
- RFN: 80947
- Chip: 33280
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Release_REQ
- Source: ts_CPHY_TrChRelNonDch LINE 1
- Message Structure:
CPHY_TrCH_Release_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 8
. TrChConfigType
- Constraint:
ca_PHY_RelReqNonDch
- BinaryMessage:
30 08 02 01 00 02 01 08 05 00

- No.: 3379
- Timestamp: 17:30:10:740_0
- RFN: 80951
- Chip: 11776
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Release_CNF
- Source: ts_CPHY_TrChRelNonDch LINE 2
- Message Structure:
CPHY_TrCH_Release_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 8
- Constraint:
ca_PHY_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 08

- No.: 3382
- Timestamp: 17:30:10:741_2
- RFN: 80951
- Chip: 14848
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 7
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 07

- No.: 3386
- Timestamp: 17:30:10:744_0
- RFN: 80951
- Chip: 26880
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 7
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 07

- No.: 3389
- Timestamp: 17:30:10:745_1
- RFN: 80951
- Chip: 29440
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 8
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 08

- No.: 3393
- Timestamp: 17:30:10:800_0
- RFN: 80957
- Chip: 12032
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 8
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 08

- No.: 3396
- Timestamp: 17:30:10:801_1
- RFN: 80957
- Chip: 15360
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -2
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 00 02 01 fe 0a 01 00 05 00

- No.: 3400
- Timestamp: 17:30:10:804_0
- RFN: 80957
- Chip: 25088
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 fe

- No.: 3403
- Timestamp: 17:30:10:805_0
- RFN: 80957
- Chip: 28672
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_CMAC_Rel LINE 1
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 5
. (RatType)ratType[0] = 0
. configMessage
- Constraint:
cas_MAC_Rel
- BinaryMessage:
30 0b 02 01 00 02 01 05 0a 01 00 05 00

- No.: 3407
- Timestamp: 17:30:10:807_0
- RFN: 80957
- Chip: 37632
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_CMAC_Rel LINE 2
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 5
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 05

- No.: 3410
- Timestamp: 17:30:10:807_3
- RFN: 80958
- Chip: 1792
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Release_REQ
- Source: ts_CPHY_TrChRelNonDch LINE 1
- Message Structure:
CPHY_TrCH_Release_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 5
. TrChConfigType
- Constraint:
ca_PHY_RelReqNonDch
- BinaryMessage:
30 08 02 01 00 02 01 05 05 00

- No.: 3414
- Timestamp: 17:30:10:812_0
- RFN: 80958
- Chip: 19712
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Release_CNF
- Source: ts_CPHY_TrChRelNonDch LINE 2
- Message Structure:
CPHY_TrCH_Release_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 5
- Constraint:
ca_PHY_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 05

- No.: 3417
- Timestamp: 17:30:10:813_0
- RFN: 80958
- Chip: 22784
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 6
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 06

- No.: 3421
- Timestamp: 17:30:10:817_0
- RFN: 80959
- Chip: 256
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 6
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 06

- No.: 3424
- Timestamp: 17:30:10:818_0
- RFN: 80959
- Chip: 3328
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 5
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 05

- No.: 3428
- Timestamp: 17:30:10:823_0
- RFN: 80959
- Chip: 23808
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 5
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 05

- No.: 3433
- Timestamp: 17:30:10:824_2
- RFN: 80959
- Chip: 27904
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 00 02 01 ff 0a 01 00 05 00

- No.: 3437
- Timestamp: 17:30:10:827_0
- RFN: 80959
- Chip: 37888
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 3440
- Timestamp: 17:30:10:828_0
- RFN: 80960
- Chip: 2816
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_CMAC_Rel LINE 1
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 4
. (RatType)ratType[0] = 0
. configMessage
- Constraint:
cas_MAC_Rel
- BinaryMessage:
30 0b 02 01 00 02 01 04 0a 01 00 05 00

- No.: 3444
- Timestamp: 17:30:10:832_0
- RFN: 80960
- Chip: 19200
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_CMAC_Rel LINE 2
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 4
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 04

- No.: 3447
- Timestamp: 17:30:10:833_0
- RFN: 80960
- Chip: 22272
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Release_REQ
- Source: ts_CPHY_TrChRelNonDch LINE 1
- Message Structure:
CPHY_TrCH_Release_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 4
. TrChConfigType
- Constraint:
ca_PHY_RelReqNonDch
- BinaryMessage:
30 08 02 01 00 02 01 04 05 00

- No.: 3451
- Timestamp: 17:30:10:837_0
- RFN: 80960
- Chip: 37120
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Release_CNF
- Source: ts_CPHY_TrChRelNonDch LINE 2
- Message Structure:
CPHY_TrCH_Release_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 4
- Constraint:
ca_PHY_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 04

- No.: 3454
- Timestamp: 17:30:10:837_3
- RFN: 80961
- Chip: 1536
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 2
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 02

- No.: 3458
- Timestamp: 17:30:10:841_0
- RFN: 80961
- Chip: 16384
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 2
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 02

- No.: 3461
- Timestamp: 17:30:10:842_1
- RFN: 80961
- Chip: 18944
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 1
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 01

- No.: 3465
- Timestamp: 17:30:10:846_0
- RFN: 80961
- Chip: 34048
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 1
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 01

- No.: 3468
- Timestamp: 17:30:10:847_0
- RFN: 80961
- Chip: 36864
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 4
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 04

- No.: 3472
- Timestamp: 17:30:10:851_0
- RFN: 80962
- Chip: 16128
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 4
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 04

- No.: 3475
- Timestamp: 17:30:10:852_0
- RFN: 80962
- Chip: 18944
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 0
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 00

- No.: 3479
- Timestamp: 17:30:10:855_0
- RFN: 80962
- Chip: 33280
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 0
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 00

- No.: 3546
- Timestamp: 17:30:10:864_0
- RFN: 80963
- Chip: 25856
- Event: Log
- PCO: VERDICT
- Message: PASS
- Source: tc_12_4_1_4c2 LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage: