| NAS_wk34-tc_12_4_1_4c2ps_2004-10-05_14.39.07

#### MMI_CmdReq

RRC |  | LLA | @ 00:00:06.050

| Message Details:
| MMI_CmdReq:
cmd (IA5String): | Please set UE in operation mode A (to support simulataneous CS and PS services)

#### CPHY INI REQ

RRC |  | PHY | @ 00:00:06.140

| Message Details:
RAN Protocol Specification: | 2003-03 R99
| Physical Layer Parameters:
Timing: | Output
Clock: | Output
ISDN Board: | ISDN
| Layer 2 Parameters:
TM bit mode: | enabled

#### CPHY INI CNF

PHY |  | RRC | @ 00:00:06.960

| Message Details:
CAPI Version: | 2.10E1_CIPHER
Release: | MX785201A_2_10E1_A_CT_SEP04_C_CIPHER
| MD8480 pool:
| BTS Group 1:
Software: | V5.10a_Cipher
FPGA: | V5.10
| Hardware Slots:
0: | TIMING GENERATOR
1: | TX BASEBAND
2: | TX BASEBAND
3: | TX BASEBAND
4: | FRAME CODER
5: | FRAME CODER
6: | RX BASEBAND
9: | ISDN V5.10a
10: | RX BASEBAND
12: | FRAME DECODER
13: | VOICE CODEC
14: | TDMA V5.10a
15: | CPU
| Options:
0: | Tx Diversity
1: | Compressed Mode
2: | Integrity & Ciphering
3: | V5.00
4: | Customer1
5: | TS34.121
6: | Router Connection
7: | CSD
| Physical Layer Parameters:
Timing: | Output
Clock: | Output
ISDN Board: | ISDN

#### MMI_CmdCnf

LLA |  | RRC | @ 00:00:07.110

| Message Details:
| MMI_CmdCnf:
result: | true
resultString (IA5String): | Omit

#### MMI_CmdReq

RRC |  | LLA | @ 00:00:07.110

| Message Details:
| MMI_CmdReq:
cmd (IA5String): | Please switch off the UE

#### MMI_CmdCnf

LLA |  | RRC | @ 00:00:07.610

| Message Details:
| MMI_CmdCnf:
result: | true
resultString (IA5String): | Omit

#### CPHY_Ini_REQ

RRC |  | LLA | @ 00:00:07.610

| Message Details:
CPHY_Ini_REQ: | defaultRadioEnvironment

#### CPHY BTS Configuration REQ

LLA |  | PHY | @ 00:00:08.360

| BTS unit: |  | 1:1
| CFN: |  | 77

| Message Details:
| Configuration Parameters:
Power Mode: | Normal Power Mode
RF Connector: | Main
Baseband Adder: | Off
LVDS: | Off
Timing: | 0
Delta Frequency: | 0
Delta Phase: | 0
| Downlink Parameters:
Frequency: | 2140000000
| Uplink Parameters:
Frequency: | 1950000000
| Tx Parameters:
Baseband Connector: | Analogue
Baseband Delay: | Not Used
| CCH Parameters:
Coder: | Tx Coder1 #1
Baseband: | Tx Baseband1
RF: | Tx RF #1
| DCH Parameters:
Coder: | Tx Coder1 #2
Baseband: | Tx Baseband1
RF: | Tx RF #1
| Rx Parameters:
Baseband Connector: | RF
RxMode: | Simultaneous PRACH/UL_DPCH
| CCH Parameters:
Coder: | Rx Decoder1 #1
Baseband: | Rx Baseband1
RF: | Rx RF #1
| DCH Parameters:
Coder: | Rx Decoder1 #2
Baseband: | Rx Baseband1
RF: | Rx RF #1

#### CPHY BTS Configuration CNF

PHY |  | LLA | @ 00:00:08.360

| BTS unit: |  | 1:1
| CFN: |  | 77

| Message Details:

#### CPHY BTS Configuration REQ

LLA |  | PHY | @ 00:00:08.370

| BTS unit: |  | 1:2
| CFN: |  | 78

| Message Details:
| Configuration Parameters:
Power Mode: | Normal Power Mode
RF Connector: | Main
Baseband Adder: | On
LVDS: | Off
Timing: | 0
Delta Frequency: | 0
Delta Phase: | 0
| Downlink Parameters:
Frequency: | 2140000000
| Uplink Parameters:
Frequency: | 1950000000
| Tx Parameters:
Baseband Connector: | Analogue
Baseband Delay: | Not Used
| CCH Parameters:
Coder: | Tx Coder2 #1
Baseband: | Tx Baseband2
RF: | Tx RF #2
| DCH Parameters:
Coder: | Tx Coder1 #2
Baseband: | Tx Baseband2
RF: | Tx RF #2
| Rx Parameters:
Baseband Connector: | RF
RxMode: | Simultaneous PRACH/UL_DPCH
| CCH Parameters:
Coder: | Rx Decoder1 #1
Baseband: | Rx Baseband2
RF: | Rx RF #2
| DCH Parameters:
Coder: | Rx Decoder1 #2
Baseband: | Rx Baseband2
RF: | Rx RF #2

#### CPHY BTS Configuration REQ

LLA |  | PHY | @ 00:00:08.370

| BTS unit: |  | 1:3
| CFN: |  | 78

| Message Details:
| Configuration Parameters:
Power Mode: | Normal Power Mode
RF Connector: | Main
Baseband Adder: | Off
LVDS: | Off
Timing: | 0
Delta Frequency: | 0
Delta Phase: | 0
| Downlink Parameters:
Frequency: | 2140000000
| Uplink Parameters:
Frequency: | 1950000000
| Tx Parameters:
Baseband Connector: | Not Connected
Baseband Delay: | Not Used
| CCH Parameters:
Coder: | Tx Coder2 #2
Baseband: | Tx Baseband3
RF: | Tx RF #2
| DCH Parameters:
Coder: | Tx Coder1 #2
Baseband: | Tx Baseband3
RF: | Tx RF #2
| Rx Parameters:
Baseband Connector: | Not Connected
RxMode: | Single PRACH/UL_DPCH
| CCH Parameters:
Coder: | Not Used
Baseband: | Not Used
RF: | Not Used
| DCH Parameters:
Coder: | Not Used
Baseband: | Not Used
RF: | Not Used

#### CPHY BTS Configuration CNF

PHY |  | LLA | @ 00:00:08.370

| BTS unit: |  | 1:2
| CFN: |  | 78

| Message Details:

#### CPHY BTS Attenuation REQ

LLA |  | PHY | @ 00:00:08.380

| BTS unit: |  | 1:1
| CFN: |  | 79

| Message Details:
| Configuration Parameters:
Tx Attenuation In dB: | 5
Rx Reference Power In dBm: | 0

#### CPHY BTS Configuration CNF

PHY |  | LLA | @ 00:00:08.380

| BTS unit: |  | 1:3
| CFN: |  | 79

| Message Details:

#### CPHY BTS Attenuation CNF

PHY |  | LLA | @ 00:00:08.390

| BTS unit: |  | 1:1
| CFN: |  | 80

| Message Details:

#### CPHY BTS Attenuation REQ

LLA |  | PHY | @ 00:00:08.400

| BTS unit: |  | 1:2
| CFN: |  | 81

| Message Details:
| Configuration Parameters:
Tx Attenuation In dB: | 5
Rx Reference Power In dBm: | 0

#### CPHY BTS Attenuation CNF

PHY |  | LLA | @ 00:00:08.400

| BTS unit: |  | 1:2
| CFN: |  | 81

| Message Details:

#### CPHY_Ini_CNF

LLA |  | RRC | @ 00:00:08.470

| Message Details:
| CPHY_Ini_CNF:
confirmation: |

#### CPHY_Cell_Config_REQ

RRC |  | LLA | @ 00:00:08.470

| Cell ID: |  | 0

| Message Details:
| CPHY_Cell_Config_REQ:
cellId: | 0
tcell: | 0
sfnOffset: | 0
| frequencyInfo:
| modeSpecificInfo:
| fdd: (FrequencyInfoFDD)
uarfcn_UL (UARFCN): | Omit
uarfcn_DL (UARFCN): | 10700
primaryScramblingCode_SS: | 100
| cellTxPowerLevel:
defaultCellTxPowerLvl: |
dLTxAttenuationLevel: | 0

#### CPHY BTS Frequency REQ

LLA |  | PHY | @ 00:00:08.480

| BTS unit: |  | 1:1
| CFN: |  | 89

| Message Details:
| Configuration Parameters:
Down Link Frequency: | 2140000000
Up Link Frequency: | 1950000000

#### CPHY BTS Frequency CNF

PHY |  | LLA | @ 00:00:08.480

| BTS unit: |  | 1:1
| CFN: |  | 89

| Message Details:

#### CPHY_Cell_Config_CNF

LLA |  | RRC | @ 00:00:08.490

| Cell ID: |  | 0

| Message Details:
| CPHY_Cell_Config_CNF:
cellId: | 0

#### CPHY_RL_Setup_REQ

RRC |  | LLA | @ 00:00:08.490

| Channel ID: |  | P-CPICH
| Cell ID: |  | 0

| Message Details:
| CPHY_RL_Setup_REQ:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 0
ratType: | fdd
| setupMessage: (CphyRlSetupReq)
| physicalChannelInfo:
| primaryCPICHInfo:
dl_TxPower_PCPICH: | -60
txdiversityIndicator: | false

#### CPHY Radio Link Setup REQ

LLA |  | PHY | @ 00:00:08.490

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: P_CPICH
| CFN: |  | 90

| Message Details:
| Configuration Parameters:
Channel Offset: | 7680
Scrambling Code: | 1600
Symbol Rate: | 15k
Channelization Code: | 0
Adjust Time: | 0
Power in dBm: | -40
Tx Diversity: | Off
NumOfDpdch: | 0

#### CPHY Radio Link Setup CNF

PHY |  | LLA | @ 00:00:08.490

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: P_CPICH
| CFN: |  | 90

| Message Details:

#### CPHY_RL_Setup_CNF

LLA |  | RRC | @ 00:00:08.500

| Channel ID: |  | P-CPICH
| Cell ID: |  | 0

| Message Details:
| CPHY_RL_Setup_CNF:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 0

#### CPHY_RL_Setup_REQ

RRC |  | LLA | @ 00:00:08.500

| Channel ID: |  | P-SCH
| Cell ID: |  | 0

| Message Details:
| CPHY_RL_Setup_REQ:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 1
ratType: | fdd
| setupMessage: (CphyRlSetupReq)
| physicalChannelInfo:
| primarySCHInfo:
tstdIndicator: | false
dl_TxPower: | -5

#### CPHY Radio Link Setup REQ

LLA |  | PHY | @ 00:00:08.510

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: P_SCH
| CFN: |  | 92

| Message Details:
| Configuration Parameters:
Channel Offset: | 7680
Adjust Time: | 0
Power in dBm: | -45
Tx Diversity: | Off
NumOfDpdch: | 0

#### CPHY Radio Link Setup CNF

PHY |  | LLA | @ 00:00:08.510

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: P_SCH
| CFN: |  | 92

| Message Details:

#### CPHY_RL_Setup_CNF

LLA |  | RRC | @ 00:00:08.520

| Channel ID: |  | P-SCH
| Cell ID: |  | 0

| Message Details:
| CPHY_RL_Setup_CNF:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 1

#### CPHY_RL_Setup_REQ

RRC |  | LLA | @ 00:00:08.520

| Channel ID: |  | S-SCH
| Cell ID: |  | 0

| Message Details:
| CPHY_RL_Setup_REQ:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 2
ratType: | fdd
| setupMessage: (CphyRlSetupReq)
| physicalChannelInfo:
| secondarySCHInfo:
tstdIndicator: | false
dl_TxPower: | -5

#### CPHY Radio Link Setup REQ

LLA |  | PHY | @ 00:00:08.520

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: S_SCH
| CFN: |  | 93

| Message Details:
| Configuration Parameters:
Channel Offset: | 7680
Adjust Time: | 0
Power in dBm: | -45
Tx Diversity: | Off
NumOfDpdch: | 0

#### CPHY Radio Link Setup CNF

PHY |  | LLA | @ 00:00:08.520

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: S_SCH
| CFN: |  | 93

| Message Details:

#### CPHY_RL_Setup_CNF

LLA |  | RRC | @ 00:00:08.540

| Channel ID: |  | S-SCH
| Cell ID: |  | 0

| Message Details:
| CPHY_RL_Setup_CNF:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 2

#### CPHY_RL_Setup_REQ

RRC |  | LLA | @ 00:00:08.540

| Channel ID: |  | P-CCPCH
| Cell ID: |  | 0

| Message Details:
| CPHY_RL_Setup_REQ:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 4
ratType: | fdd
| setupMessage: (CphyRlSetupReq)
| physicalChannelInfo:
| primaryCCPCHInfo:
sttd_Indicator: | false
dl_TxPower: | -2

#### CPHY Radio Link Setup REQ

LLA |  | PHY | @ 00:00:08.540

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: P_CCPCH
| CFN: |  | 95

| Message Details:
| Configuration Parameters:
Channel Offset: | 7680
SFN Offset: | 0
Scrambling Code: | 1600
Symbol Rate: | 15k
Channelization Code: | 1
Adjust Time: | 0
Power in dBm: | -42
Tx Diversity: | Off
NumOfDpdch: | 1

#### CPHY Radio Link Setup CNF

PHY |  | LLA | @ 00:00:08.540

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: P_CCPCH
| CFN: |  | 95

| Message Details:

#### CPHY_RL_Setup_CNF

LLA |  | RRC | @ 00:00:08.550

| Channel ID: |  | P-CCPCH
| Cell ID: |  | 0

| Message Details:
| CPHY_RL_Setup_CNF:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 4

#### CPHY_TrCH_Config_REQ

RRC |  | LLA | @ 00:00:08.550

| Channel ID: |  | P-CCPCH
| Cell ID: |  | 0

| Message Details:
| CPHY_TrCH_Config_REQ:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 4
ratType: | fdd
| trchConfigType:
nonDch: |
| configMessage: (CphyTrchConfigReq)
| activationTime: (SS_ActivationTime)
activateNow: |
| ulconnectedTrCHList: Omit
| ulTFCS: (TFCS) Omit
| dlconnectedTrCHList:
| :
trchid (TransportChannelIdentity): | 11
dl_TransportChannelType (SS_DL_TransportChannelType): | bch
| transportChannelInfo: (CommonOrDedicatedTFS)
| tti:
| tti20: (CommonOrDedicatedTF_InfoList)
| CommonOrDedicatedTF_Info:
tb_Size: | 246
| numberOfTbSizeList:
| NumberOfTransportBlocks:
one: |
| logicalChannelList:
configured: |
| semistaticTF_Information:
| channelCodingType:
convolutional (CodingRate): | half
rateMatchingAttribute: | 1
crc_Size: | crc16
| dlTFCS: (TFCS)
| normalTFCI_Signalling: (ExplicitTFCS_Configuration)
| complete: (TFCS_ReconfAdd)
| ctfcSize:
| ctfc2Bit:
| :
ctfc2: | 0
| powerOffsetInformation:
| gainFactorInformation:
| signalledGainFactors:
| modeSpecificInfo:
| fdd:
gainFactorBetaC (GainFactor): | 11
gainFactorBetaD (GainFactor): | 15
referenceTFC_ID: | 0
powerOffsetPp_m: | Omit

#### CPHY Transport Channel Configuration REQ

LLA |  | PHY | @ 00:00:08.560

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: P_CCPCH
| CFN: |  | 97

| Message Details:
| Configuration Parameters:
DTX Position: | Flexible
Second Interleave: | On
Puncture Limit: | 0
CCTrCH Length: | 270
Number Of Transport Channels: | 1
| Transport Channels:
| Item Number 0:
| Transport Channel Parameters:
| Transport Channel:
Name: | BCH
Identity: | 0
TTI (ms): | 20
EP Type: | 1/2 Rate Convolutional Coding
CRC Size: | 16
RM Attribute: | 1
First Interleave: | On
Number Of Transport Formats: | 2
| Transport Format Set:
| Transport Format 0:
Number Of Transport Blocks: | 0
Transport Block Size In Bits: | 0
| Transport Format 1:
Number Of Transport Blocks: | 1
Transport Block Size In Bits: | 246
RM Maximum Length: | 540
| Transport Format Combination Set:
Number Of Transport Format Combinations: | 2
| Transport Format Combinations 0:
Transport Format: | 0
| Transport Format Combinations 1:
Transport Format: | 1

#### CPHY Transport Channel Configuration CNF

PHY |  | LLA | @ 00:00:08.560

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: P_CCPCH
| CFN: |  | 97

| Message Details:

#### CPHY_TrCH_Config_CNF

LLA |  | RRC | @ 00:00:08.580

| Channel ID: |  | P-CCPCH
| Cell ID: |  | 0

| Message Details:
| CPHY_TrCH_Config_CNF:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 4

#### CMAC_Config_REQ

RRC |  | LLA | @ 00:00:08.580

| Channel ID: |  | P-CCPCH
| Cell ID: |  | 0

| Message Details:
| CMAC_Config_REQ:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 4
ratType: | fdd
| configMessage:
| setup: (CmacConfigReq)
| activationTime: (SS_ActivationTime)
activateNow: |
| uE_Info:
| u_RNTI: Omit
c_RNTI: | Omit
| trCHInfo:
| ulconnectedTrCHList: Omit
| ulTFCS: (TFCS) Omit
| dlconnectedTrCHList:
| :
trchid (TransportChannelIdentity): | 11
| transportChannelInfo: (CommonOrDedicatedTFS)
| tti:
| tti20: (CommonOrDedicatedTF_InfoList)
| CommonOrDedicatedTF_Info:
tb_Size: | 246
| numberOfTbSizeList:
| NumberOfTransportBlocks:
one: |
| logicalChannelList:
configured: |
| semistaticTF_Information:
| channelCodingType:
convolutional (CodingRate): | half
rateMatchingAttribute: | 1
crc_Size: | crc16
| dlTFCS: (TFCS)
| normalTFCI_Signalling: (ExplicitTFCS_Configuration)
| complete: (TFCS_ReconfAdd)
| ctfcSize:
| ctfc2Bit:
| :
ctfc2: | 0
| powerOffsetInformation:
| gainFactorInformation:
| signalledGainFactors:
| modeSpecificInfo:
| fdd:
gainFactorBetaC (GainFactor): | 11
gainFactorBetaD (GainFactor): | 15
referenceTFC_ID: | 0
powerOffsetPp_m: | Omit
| trCH_LogCHMapping: (TrCH_LogCHMappingList1)
| ulconnectedTrCHList: Omit
| dlconnectedTrCHList:
| :
trchid (TransportChannelIdentity): | 11
| trCH_LogCHMappingList:
| TrCH_LogicalChannelMapping:
| logicalChannel_Mapping:
| dl_LogicalChannelMapping: (SS_DL_LogicalChannelMapping)
macHeaderManipulation (MAC_HeaderManipulation): | normalMacHeader
dl_TransportChannelType (SS_DL_TransportChannelType): | bch
logicalChannelIdentity: | 1
logicalChannelType: | bCCH
| rlc_SizeList:
configured: |
mac_LogicalChannelPriority: | 1
rB_Identity: | -1
cn_DomainIdentity: | Omit

#### CMAC Configuration REQ

LLA |  | MAC | @ 00:00:08.590

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: P_CCPCH
| CFN: |  | 100

| Message Details:
| Configuration Parameters:
Number Of Transport Channels: | 1
| Transport Channels:
| Item Number 0:
| Transport Channel Parameters:
| Transport Channel:
Name: | BCH
Identity: | 0
TTI (ms): | 20
EP Type: | 1/2 Rate Convolutional Coding
CRC Size: | 16
RM Attribute: | 1
First Interleave: | On
Number Of Transport Formats: | 2
| Transport Format Set:
| Transport Format 0:
Number Of Transport Blocks: | 0
Transport Block Size In Bits: | 0
| Transport Format 1:
Number Of Transport Blocks: | 1
Transport Block Size In Bits: | 246
Number Of Logical Channels: | 1
| Logical Channels:
| Item Number 0:
| Logical Channel:
Name: | BCCH
Identity: | 0
Priority: | 1
CT Length: | 0
CT Value: | 0
TCTF Length: | 0
TCTF Value: | 0
UE ID Type: | Not used
UE ID: | 0
Active Flag: | 1
| Transport Format Combination Set:
Number Of Transport Format Combinations: | 2
| Transport Format Combinations 0:
Transport Format: | 0
| Transport Format Combinations 1:
Transport Format: | 1

#### CMAC Configuration CNF

MAC |  | LLA | @ 00:00:08.590

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: P_CCPCH
| CFN: |  | 100

| Message Details:

#### CMAC_Config_CNF

LLA |  | RRC | @ 00:00:08.600

| Channel ID: |  | P-CCPCH
| Cell ID: |  | 0

| Message Details:
| CMAC_Config_CNF:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 4

#### CPHY_RL_Setup_REQ

RRC |  | LLA | @ 00:00:08.600

| Channel ID: |  | S-CCPCH#1
| Cell ID: |  | 0

| Message Details:
| CPHY_RL_Setup_REQ:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 5
ratType: | fdd
| setupMessage: (CphyRlSetupReq)
| physicalChannelInfo:
| secondaryCCPCHInfo:
scramblingCode: | 0
| dl_ChannelizationCode: (SF256_AndCodeNumber)
sf64: | 1
sCCPCHSlotFormat: | 8
timingOffset: | 0
positionFixedOrFlexible: | flexible
sttd_Indicator: | false
dl_TxPower: | -2
powerOffsetOfTFCI_PO1: | 6
powerOffsetOfPILOT_PO3: | 6

#### CPHY Radio Link Setup REQ

LLA |  | PHY | @ 00:00:08.600

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: S_CCPCH
| CFN: |  | 101

| Message Details:
| Configuration Parameters:
Channel Offset: | 7680
Scrambling Code: | 1600
Symbol Rate: | 60k
Channelization Code: | 1
Adjust Time: | 0
Power in dBm: | -42
Tx Diversity: | Off
Slot Format: | 8
NumOfDpdch: | 1

#### CPHY Radio Link Setup CNF

PHY |  | LLA | @ 00:00:08.600

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: S_CCPCH
| CFN: |  | 101

| Message Details:

#### CPHY_RL_Setup_CNF

LLA |  | RRC | @ 00:00:08.610

| Channel ID: |  | S-CCPCH#1
| Cell ID: |  | 0

| Message Details:
| CPHY_RL_Setup_CNF:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 5

#### CPHY_TrCH_Config_REQ

RRC |  | LLA | @ 00:00:08.610

| Channel ID: |  | S-CCPCH#1
| Cell ID: |  | 0

| Message Details:
| CPHY_TrCH_Config_REQ:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 5
ratType: | fdd
| trchConfigType:
nonDch: |
| configMessage: (CphyTrchConfigReq)
| activationTime: (SS_ActivationTime)
activateNow: |
| ulconnectedTrCHList: Omit
| ulTFCS: (TFCS) Omit
| dlconnectedTrCHList:
| :
trchid (TransportChannelIdentity): | 12
dl_TransportChannelType (SS_DL_TransportChannelType): | pch
| transportChannelInfo: (CommonOrDedicatedTFS)
| tti:
| tti10: (CommonOrDedicatedTF_InfoList)
| CommonOrDedicatedTF_Info:
tb_Size: | 240
| numberOfTbSizeList:
| NumberOfTransportBlocks:
zero: |
| NumberOfTransportBlocks:
one: |
| logicalChannelList:
allSizes: |
| semistaticTF_Information:
| channelCodingType:
convolutional (CodingRate): | half
rateMatchingAttribute: | 230
crc_Size: | crc16
| :
trchid (TransportChannelIdentity): | 13
dl_TransportChannelType (SS_DL_TransportChannelType): | fach
| transportChannelInfo: (CommonOrDedicatedTFS)
| tti:
| tti10: (CommonOrDedicatedTF_InfoList)
| CommonOrDedicatedTF_Info:
tb_Size: | 168
| numberOfTbSizeList:
| NumberOfTransportBlocks:
zero: |
| NumberOfTransportBlocks:
one: |
| NumberOfTransportBlocks:
small: | 2
| logicalChannelList:
allSizes: |
| semistaticTF_Information:
| channelCodingType:
convolutional (CodingRate): | half
rateMatchingAttribute: | 220
crc_Size: | crc16
| :
trchid (TransportChannelIdentity): | 14
dl_TransportChannelType (SS_DL_TransportChannelType): | fach
| transportChannelInfo: (CommonOrDedicatedTFS)
| tti:
| tti10: (CommonOrDedicatedTF_InfoList)
| CommonOrDedicatedTF_Info:
tb_Size: | 360
| numberOfTbSizeList:
| NumberOfTransportBlocks:
zero: |
| NumberOfTransportBlocks:
one: |
| logicalChannelList:
allSizes: |
| semistaticTF_Information:
| channelCodingType:
turbo: |
rateMatchingAttribute: | 130
crc_Size: | crc16
| dlTFCS: (TFCS)
| normalTFCI_Signalling: (ExplicitTFCS_Configuration)
| complete: (TFCS_ReconfAdd)
| ctfcSize:
| ctfc4Bit:
| :
ctfc4: | 0
| powerOffsetInformation:
| gainFactorInformation:
computedGainFactors (ReferenceTFC_ID): | 0
powerOffsetPp_m: | Omit
| :
ctfc4: | 1
| powerOffsetInformation:
| gainFactorInformation:
computedGainFactors (ReferenceTFC_ID): | 0
powerOffsetPp_m: | Omit
| :
ctfc4: | 2
| powerOffsetInformation:
| gainFactorInformation:
computedGainFactors (ReferenceTFC_ID): | 0
powerOffsetPp_m: | Omit
| :
ctfc4: | 3
| powerOffsetInformation:
| gainFactorInformation:
computedGainFactors (ReferenceTFC_ID): | 0
powerOffsetPp_m: | Omit
| :
ctfc4: | 4
| powerOffsetInformation:
| gainFactorInformation:
computedGainFactors (ReferenceTFC_ID): | 0
powerOffsetPp_m: | Omit
| :
ctfc4: | 5
| powerOffsetInformation:
| gainFactorInformation:
computedGainFactors (ReferenceTFC_ID): | 0
powerOffsetPp_m: | Omit
| :
ctfc4: | 6
| powerOffsetInformation:
| gainFactorInformation:
computedGainFactors (ReferenceTFC_ID): | 0
powerOffsetPp_m: | Omit
| :
ctfc4: | 8
| powerOffsetInformation:
| gainFactorInformation:
| signalledGainFactors:
| modeSpecificInfo:
| fdd:
gainFactorBetaC (GainFactor): | 11
gainFactorBetaD (GainFactor): | 15
referenceTFC_ID: | 0
powerOffsetPp_m: | Omit

#### CPHY Transport Channel Configuration REQ

LLA |  | PHY | @ 00:00:08.620

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: S_CCPCH
| CFN: |  | 103

| Message Details:
| Configuration Parameters:
DTX Position: | Flexible
Second Interleave: | On
Puncture Limit: | 100
CCTrCH Length: | 1080
Number Of Transport Channels: | 3
| Transport Channels:
| Item Number 0:
| Transport Channel Parameters:
| Transport Channel:
Name: | PCH
Identity: | 0
TTI (ms): | 10
EP Type: | 1/2 Rate Convolutional Coding
CRC Size: | 16
RM Attribute: | 230
First Interleave: | On
Number Of Transport Formats: | 2
| Transport Format Set:
| Transport Format 0:
Number Of Transport Blocks: | 0
Transport Block Size In Bits: | 240
| Transport Format 1:
Number Of Transport Blocks: | 1
Transport Block Size In Bits: | 240
RM Maximum Length: | 457
| Item Number 1:
| Transport Channel Parameters:
| Transport Channel:
Name: | FACH
Identity: | 0
TTI (ms): | 10
EP Type: | 1/2 Rate Convolutional Coding
CRC Size: | 16
RM Attribute: | 220
First Interleave: | On
Number Of Transport Formats: | 3
| Transport Format Set:
| Transport Format 0:
Number Of Transport Blocks: | 0
Transport Block Size In Bits: | 168
| Transport Format 1:
Number Of Transport Blocks: | 1
Transport Block Size In Bits: | 168
| Transport Format 2:
Number Of Transport Blocks: | 2
Transport Block Size In Bits: | 168
RM Maximum Length: | 623
| Item Number 2:
| Transport Channel Parameters:
| Transport Channel:
Name: | FACH
Identity: | 1
TTI (ms): | 10
EP Type: | Turbo Coding
CRC Size: | 16
RM Attribute: | 130
First Interleave: | On
Number Of Transport Formats: | 2
| Transport Format Set:
| Transport Format 0:
Number Of Transport Blocks: | 0
Transport Block Size In Bits: | 360
| Transport Format 1:
Number Of Transport Blocks: | 1
Transport Block Size In Bits: | 360
RM Maximum Length: | 558
| Transport Format Combination Set:
Number Of Transport Format Combinations: | 8
| Transport Format Combinations 0:
Transport Format: | 0
Transport Format: | 0
Transport Format: | 0
| Transport Format Combinations 1:
Transport Format: | 1
Transport Format: | 0
Transport Format: | 0
| Transport Format Combinations 2:
Transport Format: | 0
Transport Format: | 1
Transport Format: | 0
| Transport Format Combinations 3:
Transport Format: | 1
Transport Format: | 1
Transport Format: | 0
| Transport Format Combinations 4:
Transport Format: | 0
Transport Format: | 2
Transport Format: | 0
| Transport Format Combinations 5:
Transport Format: | 1
Transport Format: | 2
Transport Format: | 0
| Transport Format Combinations 6:
Transport Format: | 0
Transport Format: | 0
Transport Format: | 1
| Transport Format Combinations 7:
Transport Format: | 0
Transport Format: | 1
Transport Format: | 1

#### CPHY Transport Channel Configuration CNF

PHY |  | LLA | @ 00:00:08.620

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: S_CCPCH
| CFN: |  | 103

| Message Details:

#### CPHY_TrCH_Config_CNF

LLA |  | RRC | @ 00:00:08.630

| Channel ID: |  | S-CCPCH#1
| Cell ID: |  | 0

| Message Details:
| CPHY_TrCH_Config_CNF:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 5

#### CMAC_Config_REQ

RRC |  | LLA | @ 00:00:08.630

| Channel ID: |  | S-CCPCH#1
| Cell ID: |  | 0

| Message Details:
| CMAC_Config_REQ:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 5
ratType: | fdd
| configMessage:
| setup: (CmacConfigReq)
| activationTime: (SS_ActivationTime)
activateNow: |
| uE_Info:
| u_RNTI: Omit
c_RNTI: | Omit
| trCHInfo:
| ulconnectedTrCHList: Omit
| ulTFCS: (TFCS) Omit
| dlconnectedTrCHList:
| :
trchid (TransportChannelIdentity): | 12
| transportChannelInfo: (CommonOrDedicatedTFS)
| tti:
| tti10: (CommonOrDedicatedTF_InfoList)
| CommonOrDedicatedTF_Info:
tb_Size: | 240
| numberOfTbSizeList:
| NumberOfTransportBlocks:
zero: |
| NumberOfTransportBlocks:
one: |
| logicalChannelList:
allSizes: |
| semistaticTF_Information:
| channelCodingType:
convolutional (CodingRate): | half
rateMatchingAttribute: | 230
crc_Size: | crc16
| :
trchid (TransportChannelIdentity): | 13
| transportChannelInfo: (CommonOrDedicatedTFS)
| tti:
| tti10: (CommonOrDedicatedTF_InfoList)
| CommonOrDedicatedTF_Info:
tb_Size: | 168
| numberOfTbSizeList:
| NumberOfTransportBlocks:
zero: |
| NumberOfTransportBlocks:
one: |
| NumberOfTransportBlocks:
small: | 2
| logicalChannelList:
allSizes: |
| semistaticTF_Information:
| channelCodingType:
convolutional (CodingRate): | half
rateMatchingAttribute: | 220
crc_Size: | crc16
| :
trchid (TransportChannelIdentity): | 14
| transportChannelInfo: (CommonOrDedicatedTFS)
| tti:
| tti10: (CommonOrDedicatedTF_InfoList)
| CommonOrDedicatedTF_Info:
tb_Size: | 360
| numberOfTbSizeList:
| NumberOfTransportBlocks:
zero: |
| NumberOfTransportBlocks:
one: |
| logicalChannelList:
allSizes: |
| semistaticTF_Information:
| channelCodingType:
turbo: |
rateMatchingAttribute: | 130
crc_Size: | crc16
| dlTFCS: (TFCS)
| normalTFCI_Signalling: (ExplicitTFCS_Configuration)
| complete: (TFCS_ReconfAdd)
| ctfcSize:
| ctfc4Bit:
| :
ctfc4: | 0
| powerOffsetInformation:
| gainFactorInformation:
computedGainFactors (ReferenceTFC_ID): | 0
powerOffsetPp_m: | Omit
| :
ctfc4: | 1
| powerOffsetInformation:
| gainFactorInformation:
computedGainFactors (ReferenceTFC_ID): | 0
powerOffsetPp_m: | Omit
| :
ctfc4: | 2
| powerOffsetInformation:
| gainFactorInformation:
computedGainFactors (ReferenceTFC_ID): | 0
powerOffsetPp_m: | Omit
| :
ctfc4: | 3
| powerOffsetInformation:
| gainFactorInformation:
computedGainFactors (ReferenceTFC_ID): | 0
powerOffsetPp_m: | Omit
| :
ctfc4: | 4
| powerOffsetInformation:
| gainFactorInformation:
computedGainFactors (ReferenceTFC_ID): | 0
powerOffsetPp_m: | Omit
| :
ctfc4: | 5
| powerOffsetInformation:
| gainFactorInformation:
computedGainFactors (ReferenceTFC_ID): | 0
powerOffsetPp_m: | Omit
| :
ctfc4: | 6
| powerOffsetInformation:
| gainFactorInformation:
computedGainFactors (ReferenceTFC_ID): | 0
powerOffsetPp_m: | Omit
| :
ctfc4: | 8
| powerOffsetInformation:
| gainFactorInformation:
| signalledGainFactors:
| modeSpecificInfo:
| fdd:
gainFactorBetaC (GainFactor): | 11
gainFactorBetaD (GainFactor): | 15
referenceTFC_ID: | 0
powerOffsetPp_m: | Omit
| trCH_LogCHMapping: (TrCH_LogCHMappingList1)
| ulconnectedTrCHList: Omit
| dlconnectedTrCHList:
| :
trchid (TransportChannelIdentity): | 12
| trCH_LogCHMappingList:
| TrCH_LogicalChannelMapping:
| logicalChannel_Mapping:
| dl_LogicalChannelMapping: (SS_DL_LogicalChannelMapping)
macHeaderManipulation (MAC_HeaderManipulation): | normalMacHeader
dl_TransportChannelType (SS_DL_TransportChannelType): | pch
logicalChannelIdentity: | 1
logicalChannelType: | pCCH
| rlc_SizeList:
configured: |
mac_LogicalChannelPriority: | 1
rB_Identity: | -2
cn_DomainIdentity: | Omit
| :
trchid (TransportChannelIdentity): | 13
| trCH_LogCHMappingList:
| TrCH_LogicalChannelMapping:
| logicalChannel_Mapping:
| dl_LogicalChannelMapping: (SS_DL_LogicalChannelMapping)
macHeaderManipulation (MAC_HeaderManipulation): | normalMacHeader
dl_TransportChannelType (SS_DL_TransportChannelType): | fach
logicalChannelIdentity: | 5
logicalChannelType: | cCCH
| rlc_SizeList:
configured: |
mac_LogicalChannelPriority: | 1
rB_Identity: | 0
cn_DomainIdentity: | Omit

#### CMAC_Config_CNF

LLA |  | RRC | @ 00:00:08.640

| Channel ID: |  | S-CCPCH#1
| Cell ID: |  | 0

| Message Details:
| CMAC_Config_CNF:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 5

#### CPHY_RL_Setup_REQ

RRC |  | LLA | @ 00:00:08.640

| Channel ID: |  | PICH#1
| Cell ID: |  | 0

| Message Details:
| CPHY_RL_Setup_REQ:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 6
ratType: | fdd
| setupMessage: (CphyRlSetupReq)
| physicalChannelInfo:
| pICHInfo:
| pichinfo: (PICH_Info)
| fdd:
channelisationCode256: | 2
pi_CountPerFrame: | e18
sttd_Indicator: | false
dl_TxPower (PICH_PowerOffset): | -5
sccpchId_associated: | 5

#### CPHY Radio Link Setup REQ

LLA |  | PHY | @ 00:00:08.650

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: PICH
| CFN: |  | 106

| Message Details:
| Configuration Parameters:
Channel Offset: | 0
Scrambling Code: | 1600
Symbol Rate: | 15k
Channelization Code: | 2
Adjust Time: | 0
Power in dBm: | -45
Tx Diversity: | Off
NumOfDpdch: | 0
Np: | 18

#### CPHY Radio Link Setup CNF

PHY |  | LLA | @ 00:00:08.650

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: PICH
| CFN: |  | 106

| Message Details:

#### CPHY_RL_Setup_CNF

LLA |  | RRC | @ 00:00:08.660

| Channel ID: |  | PICH#1
| Cell ID: |  | 0

| Message Details:
| CPHY_RL_Setup_CNF:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 6

#### CPHY_RL_Setup_REQ

RRC |  | LLA | @ 00:00:08.660

| Channel ID: |  | AICH#1
| Cell ID: |  | 0

| Message Details:
| CPHY_RL_Setup_REQ:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 7
ratType: | fdd
| setupMessage: (CphyRlSetupReq)
| physicalChannelInfo:
| aICHInfo:
| aichinfo: (AICH_Info)
channelisationCode256: | 3
sttd_Indicator: | false
aich_TransmissionTiming: | e0
dl_TxPower (AICH_PowerOffset): | -5

#### CPHY Radio Link Setup REQ

LLA |  | PHY | @ 00:00:08.660

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: AICH
| CFN: |  | 107

| Message Details:
| Configuration Parameters:
Channel Offset: | 7680
Scrambling Code: | 1600
Symbol Rate: | 15k
Channelization Code: | 3
Adjust Time: | 0
Power in dBm: | -45
Tx Diversity: | Off
AICH Transmission Timing: | 3 Access Slots
AICH Polarity: | Positive
NumOfDpdch: | 0

#### CPHY Radio Link Setup CNF

PHY |  | LLA | @ 00:00:08.660

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: AICH
| CFN: |  | 107

| Message Details:

#### CPHY_RL_Setup_CNF

LLA |  | RRC | @ 00:00:08.680

| Channel ID: |  | AICH#1
| Cell ID: |  | 0

| Message Details:
| CPHY_RL_Setup_CNF:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 7

#### CPHY_RL_Setup_REQ

RRC |  | LLA | @ 00:00:08.680

| Channel ID: |  | PRACH#1
| Cell ID: |  | 0

| Message Details:
| CPHY_RL_Setup_REQ:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 8
ratType: | fdd
| setupMessage: (CphyRlSetupReq)
| physicalChannelInfo:
| pRACHInfo:
| fdd_tdd:
| fdd:
preambleSignature (AvailableSignatures): | 0000000011111111
spreadingFactorForDataPart (SF_PRACH): | sfpr64
preambleScramblingCode (PreambleScramblingCodeWordNumber): | 0
puncturingLimit: | pl1
accessSlot (AvailableSubChannelNumbers): | 111111111111

#### CPHY_RL_Setup_CNF

LLA |  | RRC | @ 00:00:08.690

| Channel ID: |  | PRACH#1
| Cell ID: |  | 0

| Message Details:
| CPHY_RL_Setup_CNF:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 8

#### CPHY_TrCH_Config_REQ

RRC |  | LLA | @ 00:00:08.690

| Channel ID: |  | PRACH#1
| Cell ID: |  | 0

| Message Details:
| CPHY_TrCH_Config_REQ:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 8
ratType: | fdd
| trchConfigType:
nonDch: |
| configMessage: (CphyTrchConfigReq)
| activationTime: (SS_ActivationTime)
activateNow: |
| ulconnectedTrCHList:
| :
trchid (TransportChannelIdentity): | 15
ul_TransportChannelType (SS_UL_TransportChannelType): | rach
| transportChannelInfo: (CommonOrDedicatedTFS)
| tti:
| tti20: (CommonOrDedicatedTF_InfoList)
| CommonOrDedicatedTF_Info:
tb_Size: | 168
| numberOfTbSizeList:
| NumberOfTransportBlocks:
one: |
| logicalChannelList:
configured: |
| CommonOrDedicatedTF_Info:
tb_Size: | 360
| numberOfTbSizeList:
| NumberOfTransportBlocks:
one: |
| logicalChannelList:
configured: |
| semistaticTF_Information:
| channelCodingType:
convolutional (CodingRate): | half
rateMatchingAttribute: | 150
crc_Size: | crc16
| ulTFCS: (TFCS)
| normalTFCI_Signalling: (ExplicitTFCS_Configuration)
| complete: (TFCS_ReconfAdd)
| ctfcSize:
| ctfc2Bit:
| :
ctfc2: | 0
| powerOffsetInformation: Omit
| :
ctfc2: | 1
| powerOffsetInformation: Omit
| dlconnectedTrCHList: Omit
| dlTFCS: (TFCS) Omit

#### CPHY Radio Link Setup REQ

LLA |  | PHY | @ 00:00:08.700

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: PRACH
| CFN: |  | 111

| Message Details:
| Configuration Parameters:
Channel Offset: | 10240
Scrambling Code: | 16778816
Symbol Rate: | 60k
Channelization Code: | 128
Adjust Time: | 0
Slot Format: | 2
NumOfDpdch: | 1

#### CPHY Radio Link Setup CNF

PHY |  | LLA | @ 00:00:08.700

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: PRACH
| CFN: |  | 111

| Message Details:

#### CPHY Transport Channel Configuration REQ

LLA |  | PHY | @ 00:00:08.730

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: PRACH
| CFN: |  | 114

| Message Details:
| Configuration Parameters:
DTX Position: | Flexible
Second Interleave: | On
Puncture Limit: | 100
CCTrCH Length: | 600
Number Of Transport Channels: | 1
| Transport Channels:
| Item Number 0:
| Transport Channel Parameters:
| Transport Channel:
Name: | RACH
Identity: | 0
TTI (ms): | 20
EP Type: | 1/2 Rate Convolutional Coding
CRC Size: | 16
RM Attribute: | 150
First Interleave: | On
Number Of Transport Formats: | 2
| Transport Format Set:
| Transport Format 0:
Number Of Transport Blocks: | 1
Transport Block Size In Bits: | 168
| Transport Format 1:
Number Of Transport Blocks: | 1
Transport Block Size In Bits: | 360
RM Maximum Length: | 600
| Transport Format Combination Set:
Number Of Transport Format Combinations: | 2
| Transport Format Combinations 0:
Transport Format: | 0
| Transport Format Combinations 1:
Transport Format: | 1

#### CPHY Transport Channel Configuration CNF

PHY |  | LLA | @ 00:00:08.740

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: PRACH
| CFN: |  | 115

| Message Details:

#### CPHY_TrCH_Config_CNF

LLA |  | RRC | @ 00:00:08.750

| Channel ID: |  | PRACH#1
| Cell ID: |  | 0

| Message Details:
| CPHY_TrCH_Config_CNF:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 8

#### CMAC_Config_REQ

RRC |  | LLA | @ 00:00:08.750

| Channel ID: |  | PRACH#1
| Cell ID: |  | 0

| Message Details:
| CMAC_Config_REQ:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 8
ratType: | fdd
| configMessage:
| setup: (CmacConfigReq)
| activationTime: (SS_ActivationTime)
activateNow: |
| uE_Info:
| u_RNTI: Omit
c_RNTI: | Omit
| trCHInfo:
| ulconnectedTrCHList:
| :
trchid (TransportChannelIdentity): | 15
| transportChannelInfo: (CommonOrDedicatedTFS)
| tti:
| tti20: (CommonOrDedicatedTF_InfoList)
| CommonOrDedicatedTF_Info:
tb_Size: | 168
| numberOfTbSizeList:
| NumberOfTransportBlocks:
one: |
| logicalChannelList:
configured: |
| CommonOrDedicatedTF_Info:
tb_Size: | 360
| numberOfTbSizeList:
| NumberOfTransportBlocks:
one: |
| logicalChannelList:
configured: |
| semistaticTF_Information:
| channelCodingType:
convolutional (CodingRate): | half
rateMatchingAttribute: | 150
crc_Size: | crc16
| ulTFCS: (TFCS)
| normalTFCI_Signalling: (ExplicitTFCS_Configuration)
| complete: (TFCS_ReconfAdd)
| ctfcSize:
| ctfc2Bit:
| :
ctfc2: | 0
| powerOffsetInformation: Omit
| :
ctfc2: | 1
| powerOffsetInformation: Omit
| dlconnectedTrCHList: Omit
| dlTFCS: (TFCS) Omit
| trCH_LogCHMapping: (TrCH_LogCHMappingList1)
| ulconnectedTrCHList:
| :
trchid (TransportChannelIdentity): | 15
| trCH_LogCHMappingList:
| TrCH_LogicalChannelMapping:
| logicalChannel_Mapping:
| ul_LogicalChannelMapping: (SS_UL_LogicalChannelMapping)
macHeaderManipulation (MAC_HeaderManipulation): | normalMacHeader
ul_TransportChannelType (SS_UL_TransportChannelType): | rach
logicalChannelIdentity: | 5
logicalChannelType: | cCCH
rB_Identity: | 0
cn_DomainIdentity: | Omit
| dlconnectedTrCHList: Omit

#### CMAC Configuration REQ

LLA |  | MAC | @ 00:00:08.760

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: PRACH
| CFN: |  | 117

| Message Details:
| Configuration Parameters:
Number Of Transport Channels: | 1
| Transport Channels:
| Item Number 0:
| Transport Channel Parameters:
| Transport Channel:
Name: | RACH
Identity: | 0
TTI (ms): | 20
EP Type: | 1/2 Rate Convolutional Coding
CRC Size: | 16
RM Attribute: | 150
First Interleave: | On
Number Of Transport Formats: | 2
| Transport Format Set:
| Transport Format 0:
Number Of Transport Blocks: | 1
Transport Block Size In Bits: | 168
| Transport Format 1:
Number Of Transport Blocks: | 1
Transport Block Size In Bits: | 360
Number Of Logical Channels: | 1
| Logical Channels:
| Item Number 0:
| Logical Channel:
Name: | CCCH
Identity: | 0
Priority: | 0
CT Length: | 0
CT Value: | 0
TCTF Length: | 2
TCTF Value: | 0
UE ID Type: | Not used
UE ID: | 0
Active Flag: | 1
| Transport Format Combination Set:
Number Of Transport Format Combinations: | 2
| Transport Format Combinations 0:
Transport Format: | 0
| Transport Format Combinations 1:
Transport Format: | 1

#### CMAC Configuration CNF

MAC |  | LLA | @ 00:00:08.760

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: PRACH
| CFN: |  | 117

| Message Details:

#### CMAC_Config_CNF

LLA |  | RRC | @ 00:00:08.770

| Channel ID: |  | PRACH#1
| Cell ID: |  | 0

| Message Details:
| CMAC_Config_CNF:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 8

#### CPHY_RL_Setup_REQ

RRC |  | LLA | @ 00:00:08.770

| Channel ID: |  | DL-DPCH#1
| Cell ID: |  | 0

| Message Details:
| CPHY_RL_Setup_REQ:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 26
ratType: | fdd
| setupMessage: (CphyRlSetupReq)
| physicalChannelInfo:
| dPCHInfo:
| ul_DPCHInfo: (UL_DPCH_Info) Omit
| dl_DPCHInfo:
| dl_CommonInformation:
| dl_DPCH_InfoCommon:
| cfnHandling:
| initialise:
cfntargetsfnframeoffset: | Omit
| modeSpecificInfo:
| fdd:
| dl_DPCH_PowerControlInfo:
| modeSpecificInfo:
| fdd:
dpc_Mode: | singleTPC
powerOffsetPilot_pdpdch: | 0
| dl_rate_matching_restriction: Omit
| spreadingFactorAndPilot: (SF512_AndPilot)
sfd128 (PilotBits128): | pb4
positionFixedOrFlexible: | fixed
tfci_Existence: | false
| modeSpecificInfo:
| fdd:
defaultDPCH_OffsetValue (DefaultDPCH_OffsetValueFDD): | 0
| dpch_CompressedModeInfo: Omit
tx_DiversityMode: | noDiversity
| ssdt_Information: Omit
| dl_DPCH_InfoPerRL:
| fdd:
pCPICH_UsageForChannelEst: | mayBeUsed
dpch_FrameOffset: | 0
| secondaryCPICH_Info: Omit
| dl_ChannelisationCodeList:
| DL_ChannelisationCode:
secondaryScramblingCode: | 1
| sf_AndCodeNumber: (SF512_AndCodeNumber)
sf128: | 0
scramblingCodeChange: | Omit
tpc_CombinationIndex: | 0
ssdt_CellIdentity: | Omit
closedLoopTimingAdjMode: | Omit
powerOffsetOfTFCI_PO1: | 0
powerOffsetOfTPC_PO2: | 0
powerOffsetOfPILOT_PO3: | 0
dl_TxPower: | -5
dl_TxPowerMax (DL_TxPower): | 15
dl_TxPowerMin (DL_TxPower): | -35

#### CPHY Radio Link Setup REQ

LLA |  | PHY | @ 00:00:08.780

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: D_DPCH
| CFN: |  | 119

| Message Details:
| Configuration Parameters:
Channel Offset: | 7680
Scrambling Code: | 1601
Symbol Rate: | 30k
Channelization Code: | 0
Adjust Time: | 0
Power in dBm: | -45
Tx Diversity: | Off
Slot Format: | 8
Number Of DPDCH: | 1
| DPDCH Parameters:
| Item Number 0:
Power in dBm: | -45
Channelization Code: | 0

#### CPHY Radio Link Setup CNF

PHY |  | LLA | @ 00:00:08.780

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: D_DPCH
| CFN: |  | 119

| Message Details:

#### CPHY_RL_Setup_CNF

LLA |  | RRC | @ 00:00:08.800

| Channel ID: |  | DL-DPCH#1
| Cell ID: |  | 0

| Message Details:
| CPHY_RL_Setup_CNF:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 26

#### CPHY_TrCH_Config_REQ

RRC |  | LLA | @ 00:00:08.800

| Channel ID: |  | DL-DPCH#1
| Cell ID: |  | 0

| Message Details:
| CPHY_TrCH_Config_REQ:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 26
ratType: | fdd
| trchConfigType:
dch: | normal
| configMessage: (CphyTrchConfigReq)
| activationTime: (SS_ActivationTime)
activateNow: |
| ulconnectedTrCHList: Omit
| ulTFCS: (TFCS) Omit
| dlconnectedTrCHList:
| :
trchid (TransportChannelIdentity): | 10
dl_TransportChannelType (SS_DL_TransportChannelType): | dch
| transportChannelInfo: (CommonOrDedicatedTFS)
| tti:
| tti10: (CommonOrDedicatedTF_InfoList)
| CommonOrDedicatedTF_Info:
tb_Size: | 148
| numberOfTbSizeList:
| NumberOfTransportBlocks:
zero: |
| NumberOfTransportBlocks:
one: |
| logicalChannelList:
allSizes: |
| semistaticTF_Information:
| channelCodingType:
convolutional (CodingRate): | third
rateMatchingAttribute: | 192
crc_Size: | crc16
| dlTFCS: (TFCS)
| normalTFCI_Signalling: (ExplicitTFCS_Configuration)
| complete: (TFCS_ReconfAdd)
| ctfcSize:
| ctfc2Bit:
| :
ctfc2: | 0
| powerOffsetInformation:
| gainFactorInformation:
computedGainFactors (ReferenceTFC_ID): | 0
powerOffsetPp_m: | Omit
| :
ctfc2: | 1
| powerOffsetInformation:
| gainFactorInformation:
| signalledGainFactors:
| modeSpecificInfo:
| fdd:
gainFactorBetaC (GainFactor): | 11
gainFactorBetaD (GainFactor): | 15
referenceTFC_ID: | 0
powerOffsetPp_m: | Omit

#### CPHY Transport Channel Configuration REQ

LLA |  | PHY | @ 00:00:08.810

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: D_DPCH
| CFN: |  | 122

| Message Details:
| Configuration Parameters:
DTX Position: | Fixed
Second Interleave: | On
Puncture Limit: | 0
CCTrCH Length: | 510
Number Of Transport Channels: | 1
| Transport Channels:
| Item Number 0:
| Transport Channel Parameters:
| Transport Channel:
Name: | D_DCH
Identity: | 0
TTI (ms): | 10
EP Type: | 1/3 Rate Convolutional Coding
CRC Size: | 16
RM Attribute: | 192
First Interleave: | On
Number Of Transport Formats: | 2
| Transport Format Set:
| Transport Format 0:
Number Of Transport Blocks: | 0
Transport Block Size In Bits: | 148
| Transport Format 1:
Number Of Transport Blocks: | 1
Transport Block Size In Bits: | 148
RM Maximum Length: | 510
| Transport Format Combination Set:
Number Of Transport Format Combinations: | 2
| Transport Format Combinations 0:
Transport Format: | 0
| Transport Format Combinations 1:
Transport Format: | 1

#### CPHY Transport Channel Configuration CNF

PHY |  | LLA | @ 00:00:08.810

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: D_DPCH
| CFN: |  | 122

| Message Details:

#### CPHY_TrCH_Config_CNF

LLA |  | RRC | @ 00:00:08.830

| Channel ID: |  | DL-DPCH#1
| Cell ID: |  | 0

| Message Details:
| CPHY_TrCH_Config_CNF:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 26

#### CMAC_Config_REQ

RRC |  | LLA | @ 00:00:08.830

| Channel ID: |  | DL-DPCH#1
| Cell ID: |  | -1

| Message Details:
| CMAC_Config_REQ:
cellId: | -1
| routingInfo:
physicalChannelIdentity: | 26
ratType: | fdd
| configMessage:
| setup: (CmacConfigReq)
| activationTime: (SS_ActivationTime)
activateNow: |
| uE_Info:
| u_RNTI: Omit
c_RNTI: | Omit
| trCHInfo:
| ulconnectedTrCHList: Omit
| ulTFCS: (TFCS) Omit
| dlconnectedTrCHList:
| :
trchid (TransportChannelIdentity): | 10
| transportChannelInfo: (CommonOrDedicatedTFS)
| tti:
| tti10: (CommonOrDedicatedTF_InfoList)
| CommonOrDedicatedTF_Info:
tb_Size: | 148
| numberOfTbSizeList:
| NumberOfTransportBlocks:
zero: |
| NumberOfTransportBlocks:
one: |
| logicalChannelList:
allSizes: |
| semistaticTF_Information:
| channelCodingType:
convolutional (CodingRate): | third
rateMatchingAttribute: | 192
crc_Size: | crc16
| dlTFCS: (TFCS)
| normalTFCI_Signalling: (ExplicitTFCS_Configuration)
| complete: (TFCS_ReconfAdd)
| ctfcSize:
| ctfc2Bit:
| :
ctfc2: | 0
| powerOffsetInformation:
| gainFactorInformation:
computedGainFactors (ReferenceTFC_ID): | 0
powerOffsetPp_m: | Omit
| :
ctfc2: | 1
| powerOffsetInformation:
| gainFactorInformation:
| signalledGainFactors:
| modeSpecificInfo:
| fdd:
gainFactorBetaC (GainFactor): | 11
gainFactorBetaD (GainFactor): | 15
referenceTFC_ID: | 0
powerOffsetPp_m: | Omit
| trCH_LogCHMapping: (TrCH_LogCHMappingList1)
| ulconnectedTrCHList: Omit
| dlconnectedTrCHList:
| :
trchid (TransportChannelIdentity): | 10
| trCH_LogCHMappingList:
| TrCH_LogicalChannelMapping:
| logicalChannel_Mapping:
| dl_LogicalChannelMapping: (SS_DL_LogicalChannelMapping)
macHeaderManipulation (MAC_HeaderManipulation): | normalMacHeader
dl_TransportChannelType (SS_DL_TransportChannelType): | dch
logicalChannelIdentity: | 1
logicalChannelType: | dCCH
| rlc_SizeList:
configured: |
mac_LogicalChannelPriority: | 1
rB_Identity: | 1
cn_DomainIdentity: | Omit
| TrCH_LogicalChannelMapping:
| logicalChannel_Mapping:
| dl_LogicalChannelMapping: (SS_DL_LogicalChannelMapping)
macHeaderManipulation (MAC_HeaderManipulation): | normalMacHeader
dl_TransportChannelType (SS_DL_TransportChannelType): | dch
logicalChannelIdentity: | 2
logicalChannelType: | dCCH
| rlc_SizeList:
configured: |
mac_LogicalChannelPriority: | 2
rB_Identity: | 2
cn_DomainIdentity: | Omit
| TrCH_LogicalChannelMapping:
| logicalChannel_Mapping:
| dl_LogicalChannelMapping: (SS_DL_LogicalChannelMapping)
macHeaderManipulation (MAC_HeaderManipulation): | normalMacHeader
dl_TransportChannelType (SS_DL_TransportChannelType): | dch
logicalChannelIdentity: | 3
logicalChannelType: | dCCH
| rlc_SizeList:
configured: |
mac_LogicalChannelPriority: | 3
rB_Identity: | 3
cn_DomainIdentity: | Omit
| TrCH_LogicalChannelMapping:
| logicalChannel_Mapping:
| dl_LogicalChannelMapping: (SS_DL_LogicalChannelMapping)
macHeaderManipulation (MAC_HeaderManipulation): | normalMacHeader
dl_TransportChannelType (SS_DL_TransportChannelType): | dch
logicalChannelIdentity: | 4
logicalChannelType: | dCCH
| rlc_SizeList:
configured: |
mac_LogicalChannelPriority: | 4
rB_Identity: | 4
cn_DomainIdentity: | Omit

#### CMAC Configuration REQ

LLA |  | MAC | @ 00:00:08.840

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: D_DPCH
| CFN: |  | 125

| Message Details:
| Configuration Parameters:
Number Of Transport Channels: | 1
| Transport Channels:
| Item Number 0:
| Transport Channel Parameters:
| Transport Channel:
Name: | D_DCH
Identity: | 0
TTI (ms): | 10
EP Type: | 1/3 Rate Convolutional Coding
CRC Size: | 16
RM Attribute: | 192
First Interleave: | On
Number Of Transport Formats: | 2
| Transport Format Set:
| Transport Format 0:
Number Of Transport Blocks: | 0
Transport Block Size In Bits: | 148
| Transport Format 1:
Number Of Transport Blocks: | 1
Transport Block Size In Bits: | 148
Number Of Logical Channels: | 4
| Logical Channels:
| Item Number 0:
| Logical Channel:
Name: | DCCH
Identity: | 1
Priority: | 1
CT Length: | 4
CT Value: | 0
TCTF Length: | 0
TCTF Value: | 0
UE ID Type: | Not used
UE ID: | 0
| Item Number 1:
| Logical Channel:
Name: | DCCH
Identity: | 2
Priority: | 2
CT Length: | 4
CT Value: | 1
TCTF Length: | 0
TCTF Value: | 0
UE ID Type: | Not used
UE ID: | 0
| Item Number 2:
| Logical Channel:
Name: | DCCH
Identity: | 3
Priority: | 3
CT Length: | 4
CT Value: | 2
TCTF Length: | 0
TCTF Value: | 0
UE ID Type: | Not used
UE ID: | 0
| Item Number 3:
| Logical Channel:
Name: | DCCH
Identity: | 4
Priority: | 4
CT Length: | 4
CT Value: | 3
TCTF Length: | 0
TCTF Value: | 0
UE ID Type: | Not used
UE ID: | 0
Active Flag: | 1
| Transport Format Combination Set:
Number Of Transport Format Combinations: | 2
| Transport Format Combinations 0:
Transport Format: | 0
| Transport Format Combinations 1:
Transport Format: | 1

#### CMAC Configuration CNF

MAC |  | LLA | @ 00:00:08.840

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: D_DPCH
| CFN: |  | 125

| Message Details:

#### CMAC_Config_CNF

LLA |  | RRC | @ 00:00:08.850

| Channel ID: |  | DL-DPCH#1
| Cell ID: |  | -1

| Message Details:
| CMAC_Config_CNF:
cellId: | -1
| routingInfo:
physicalChannelIdentity: | 26

#### CPHY_RL_Setup_REQ

RRC |  | LLA | @ 00:00:08.850

| Channel ID: |  | UL-DPCH#1
| Cell ID: |  | 0

| Message Details:
| CPHY_RL_Setup_REQ:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 20
ratType: | fdd
| setupMessage: (CphyRlSetupReq)
| physicalChannelInfo:
| dPCHInfo:
| ul_DPCHInfo: (UL_DPCH_Info)
| ul_DPCH_PowerControlInfo:
| fdd:
dpcch_PowerOffset: | -40
pc_Preamble: | 1
sRB_delay: | 7
| powerControlAlgorithm:
algorithm1 (TPC_StepSizeFDD): | 0
| modeSpecificInfo:
| fdd:
scramblingCodeType: | longSC
scramblingCode (UL_ScramblingCode): | 0
numberOfDPDCH: | Omit
spreadingFactor: | sf64
tfci_Existence: | true
numberOfFBI_Bits: | Omit
puncturingLimit: | pl1
| dl_DPCHInfo: Omit

#### CPHY_RL_Setup_CNF

LLA |  | RRC | @ 00:00:08.860

| Channel ID: |  | UL-DPCH#1
| Cell ID: |  | 0

| Message Details:
| CPHY_RL_Setup_CNF:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 20

#### CPHY_TrCH_Config_REQ

RRC |  | LLA | @ 00:00:08.860

| Channel ID: |  | UL-DPCH#1
| Cell ID: |  | 0

| Message Details:
| CPHY_TrCH_Config_REQ:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 20
ratType: | fdd
| trchConfigType:
dch: | normal
| configMessage: (CphyTrchConfigReq)
| activationTime: (SS_ActivationTime)
activateNow: |
| ulconnectedTrCHList:
| :
trchid (TransportChannelIdentity): | 5
ul_TransportChannelType (SS_UL_TransportChannelType): | dch
| transportChannelInfo: (CommonOrDedicatedTFS)
| tti:
| tti10: (CommonOrDedicatedTF_InfoList)
| CommonOrDedicatedTF_Info:
tb_Size: | 148
| numberOfTbSizeList:
| NumberOfTransportBlocks:
zero: |
| NumberOfTransportBlocks:
one: |
| logicalChannelList:
allSizes: |
| semistaticTF_Information:
| channelCodingType:
convolutional (CodingRate): | third
rateMatchingAttribute: | 192
crc_Size: | crc16
| ulTFCS: (TFCS)
| normalTFCI_Signalling: (ExplicitTFCS_Configuration)
| complete: (TFCS_ReconfAdd)
| ctfcSize:
| ctfc2Bit:
| :
ctfc2: | 0
| powerOffsetInformation: Omit
| :
ctfc2: | 1
| powerOffsetInformation: Omit
| dlconnectedTrCHList: Omit
| dlTFCS: (TFCS) Omit

#### CPHY Radio Link Setup REQ

LLA |  | PHY | @ 00:00:08.870

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: U_DPCH
| CFN: |  | 128

| Message Details:
| Configuration Parameters:
Channel Offset: | 8704
Scrambling Code: | 16777216
Symbol Rate: | 60k
Channelization Code: | 0
Adjust Time: | 0
Slot Format: | 0
Number Of DPDCH: | 1
| DPDCH Parameters:
| Item Number 0:
Channelization Code: | 16

#### CPHY Radio Link Setup CNF

PHY |  | LLA | @ 00:00:08.870

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: U_DPCH
| CFN: |  | 128

| Message Details:

#### CPHY Transport Channel Configuration REQ

LLA |  | PHY | @ 00:00:08.880

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: U_DPCH
| CFN: |  | 129

| Message Details:
| Configuration Parameters:
DTX Position: | Flexible
Second Interleave: | On
Puncture Limit: | 100
CCTrCH Length: | 600
Number Of Transport Channels: | 1
| Transport Channels:
| Item Number 0:
| Transport Channel Parameters:
| Transport Channel:
Name: | U_DCH
Identity: | 0
TTI (ms): | 10
EP Type: | 1/3 Rate Convolutional Coding
CRC Size: | 16
RM Attribute: | 192
First Interleave: | On
Number Of Transport Formats: | 2
| Transport Format Set:
| Transport Format 0:
Number Of Transport Blocks: | 0
Transport Block Size In Bits: | 148
| Transport Format 1:
Number Of Transport Blocks: | 1
Transport Block Size In Bits: | 148
RM Maximum Length: | 600
| Transport Format Combination Set:
Number Of Transport Format Combinations: | 2
| Transport Format Combinations 0:
Transport Format: | 0
| Transport Format Combinations 1:
Transport Format: | 1

#### CPHY Transport Channel Configuration CNF

PHY |  | LLA | @ 00:00:08.900

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: U_DPCH
| CFN: |  | 131

| Message Details:

#### CPHY_TrCH_Config_CNF

LLA |  | RRC | @ 00:00:08.910

| Channel ID: |  | UL-DPCH#1
| Cell ID: |  | 0

| Message Details:
| CPHY_TrCH_Config_CNF:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 20

#### CMAC_Config_REQ

RRC |  | LLA | @ 00:00:08.910

| Channel ID: |  | UL-DPCH#1
| Cell ID: |  | -1

| Message Details:
| CMAC_Config_REQ:
cellId: | -1
| routingInfo:
physicalChannelIdentity: | 20
ratType: | fdd
| configMessage:
| setup: (CmacConfigReq)
| activationTime: (SS_ActivationTime)
activateNow: |
| uE_Info:
| u_RNTI: Omit
c_RNTI: | Omit
| trCHInfo:
| ulconnectedTrCHList:
| :
trchid (TransportChannelIdentity): | 5
| transportChannelInfo: (CommonOrDedicatedTFS)
| tti:
| tti10: (CommonOrDedicatedTF_InfoList)
| CommonOrDedicatedTF_Info:
tb_Size: | 148
| numberOfTbSizeList:
| NumberOfTransportBlocks:
zero: |
| NumberOfTransportBlocks:
one: |
| logicalChannelList:
allSizes: |
| semistaticTF_Information:
| channelCodingType:
convolutional (CodingRate): | third
rateMatchingAttribute: | 192
crc_Size: | crc16
| ulTFCS: (TFCS)
| normalTFCI_Signalling: (ExplicitTFCS_Configuration)
| complete: (TFCS_ReconfAdd)
| ctfcSize:
| ctfc2Bit:
| :
ctfc2: | 0
| powerOffsetInformation: Omit
| :
ctfc2: | 1
| powerOffsetInformation: Omit
| dlconnectedTrCHList: Omit
| dlTFCS: (TFCS) Omit
| trCH_LogCHMapping: (TrCH_LogCHMappingList1)
| ulconnectedTrCHList:
| :
trchid (TransportChannelIdentity): | 5
| trCH_LogCHMappingList:
| TrCH_LogicalChannelMapping:
| logicalChannel_Mapping:
| ul_LogicalChannelMapping: (SS_UL_LogicalChannelMapping)
macHeaderManipulation (MAC_HeaderManipulation): | normalMacHeader
ul_TransportChannelType (SS_UL_TransportChannelType): | dch
logicalChannelIdentity: | 1
logicalChannelType: | dCCH
rB_Identity: | 1
cn_DomainIdentity: | Omit
| TrCH_LogicalChannelMapping:
| logicalChannel_Mapping:
| ul_LogicalChannelMapping: (SS_UL_LogicalChannelMapping)
macHeaderManipulation (MAC_HeaderManipulation): | normalMacHeader
ul_TransportChannelType (SS_UL_TransportChannelType): | dch
logicalChannelIdentity: | 2
logicalChannelType: | dCCH
rB_Identity: | 2
cn_DomainIdentity: | Omit
| TrCH_LogicalChannelMapping:
| logicalChannel_Mapping:
| ul_LogicalChannelMapping: (SS_UL_LogicalChannelMapping)
macHeaderManipulation (MAC_HeaderManipulation): | normalMacHeader
ul_TransportChannelType (SS_UL_TransportChannelType): | dch
logicalChannelIdentity: | 3
logicalChannelType: | dCCH
rB_Identity: | 3
cn_DomainIdentity: | Omit
| TrCH_LogicalChannelMapping:
| logicalChannel_Mapping:
| ul_LogicalChannelMapping: (SS_UL_LogicalChannelMapping)
macHeaderManipulation (MAC_HeaderManipulation): | normalMacHeader
ul_TransportChannelType (SS_UL_TransportChannelType): | dch
logicalChannelIdentity: | 4
logicalChannelType: | dCCH
rB_Identity: | 4
cn_DomainIdentity: | Omit
| dlconnectedTrCHList: Omit

#### CMAC Configuration REQ

LLA |  | MAC | @ 00:00:08.920

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: U_DPCH
| CFN: |  | 133

| Message Details:
| Configuration Parameters:
Number Of Transport Channels: | 1
| Transport Channels:
| Item Number 0:
| Transport Channel Parameters:
| Transport Channel:
Name: | U_DCH
Identity: | 0
TTI (ms): | 10
EP Type: | 1/3 Rate Convolutional Coding
CRC Size: | 16
RM Attribute: | 192
First Interleave: | On
Number Of Transport Formats: | 2
| Transport Format Set:
| Transport Format 0:
Number Of Transport Blocks: | 0
Transport Block Size In Bits: | 148
| Transport Format 1:
Number Of Transport Blocks: | 1
Transport Block Size In Bits: | 148
Number Of Logical Channels: | 4
| Logical Channels:
| Item Number 0:
| Logical Channel:
Name: | DCCH
Identity: | 1
Priority: | 0
CT Length: | 4
CT Value: | 0
TCTF Length: | 0
TCTF Value: | 0
UE ID Type: | Not used
UE ID: | 0
| Item Number 1:
| Logical Channel:
Name: | DCCH
Identity: | 2
Priority: | 0
CT Length: | 4
CT Value: | 1
TCTF Length: | 0
TCTF Value: | 0
UE ID Type: | Not used
UE ID: | 0
| Item Number 2:
| Logical Channel:
Name: | DCCH
Identity: | 3
Priority: | 0
CT Length: | 4
CT Value: | 2
TCTF Length: | 0
TCTF Value: | 0
UE ID Type: | Not used
UE ID: | 0
| Item Number 3:
| Logical Channel:
Name: | DCCH
Identity: | 4
Priority: | 0
CT Length: | 4
CT Value: | 3
TCTF Length: | 0
TCTF Value: | 0
UE ID Type: | Not used
UE ID: | 0
Active Flag: | 1
| Transport Format Combination Set:
Number Of Transport Format Combinations: | 2
| Transport Format Combinations 0:
Transport Format: | 0
| Transport Format Combinations 1:
Transport Format: | 1

#### CMAC Configuration CNF

MAC |  | LLA | @ 00:00:08.920

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: U_DPCH
| CFN: |  | 133

| Message Details:

#### CMAC_Config_CNF

LLA |  | RRC | @ 00:00:08.930

| Channel ID: |  | UL-DPCH#1
| Cell ID: |  | -1

| Message Details:
| CMAC_Config_CNF:
cellId: | -1
| routingInfo:
physicalChannelIdentity: | 20

#### CRLC_Config_REQ

RRC |  | LLA | @ 00:00:08.930

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CRLC_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CrlcConfigReq)
| setup: (RBInfo)
| sS_rlc_Info:
| sS_ul_RLC_Mode: (DL_RLC_Mode) Omit
| sS_dl_RLC_Mode:
dl_PayloadSize (PayloadSize): | 246
| dl_RLCModeInfo: (UL_RLC_Mode)
| ul_TM_RLC_Mode:
| transmissionRLC_Discard: Omit
segmentationIndication: | false
| rB_LogCH_Mapping:
uLlogicalChannelIdentity (LogicalChannelIdentity): | Omit
dLlogicalChannelIdentity (LogicalChannelIdentity): | 1
logicalChannelType: | Omit
cn_DomainIdentity: | Omit

#### CRLC TM Channel Establish REQ

LLA |  | RLC | @ 00:00:08.930

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCCH
| CFN: |  | 134

| Message Details:
| Configuration Parameters:
Number Of PU Sizes: | 1
| PU sizes In Bits:
Item 0: | 246

#### CRLC TM Channel Establish CNF

RLC |  | LLA | @ 00:00:08.930

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCCH
| CFN: |  | 134

| Message Details:

#### CRLC_Config_CNF

LLA |  | RRC | @ 00:00:08.940

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CRLC_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### CRLC_Config_REQ

RRC |  | LLA | @ 00:00:08.940

| Channel ID: |  | RbPcch
| Cell ID: |  | 0

| Message Details:
| CRLC_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -2
ratType: | fdd
| configMessage: (CrlcConfigReq)
| setup: (RBInfo)
| sS_rlc_Info:
| sS_ul_RLC_Mode: (DL_RLC_Mode) Omit
| sS_dl_RLC_Mode:
dl_PayloadSize (PayloadSize): | 240
| dl_RLCModeInfo: (UL_RLC_Mode)
| ul_TM_RLC_Mode:
| transmissionRLC_Discard: Omit
segmentationIndication: | false
| rB_LogCH_Mapping:
uLlogicalChannelIdentity (LogicalChannelIdentity): | Omit
dLlogicalChannelIdentity (LogicalChannelIdentity): | 1
logicalChannelType: | Omit
cn_DomainIdentity: | Omit

#### CRLC TM Channel Establish REQ

LLA |  | RLC | @ 00:00:08.940

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: PCCH
| CFN: |  | 135

| Message Details:
| Configuration Parameters:
Number Of PU Sizes: | 1
| PU sizes In Bits:
Item 0: | 240

#### CRLC TM Channel Establish CNF

RLC |  | LLA | @ 00:00:08.940

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: PCCH
| CFN: |  | 135

| Message Details:

#### CRLC_Config_CNF

LLA |  | RRC | @ 00:00:08.960

| Channel ID: |  | RbPcch
| Cell ID: |  | 0

| Message Details:
| CRLC_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -2

#### CRLC_Config_REQ

RRC |  | LLA | @ 00:00:08.960

| Channel ID: |  | Rb0
| Cell ID: |  | 0

| Message Details:
| CRLC_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | 0
ratType: | fdd
| configMessage: (CrlcConfigReq)
| setup: (RBInfo)
| sS_rlc_Info:
| sS_ul_RLC_Mode: (DL_RLC_Mode) Omit
| sS_dl_RLC_Mode:
dl_PayloadSize (PayloadSize): | 152
| dl_RLCModeInfo: (UL_RLC_Mode)
| ul_UM_RLC_Mode:
| transmissionRLC_Discard:
timerBasedNoExplicit (NoExplicitDiscard): | dt100
| rB_LogCH_Mapping:
uLlogicalChannelIdentity (LogicalChannelIdentity): | Omit
dLlogicalChannelIdentity (LogicalChannelIdentity): | 5
logicalChannelType: | Omit
cn_DomainIdentity: | Omit

#### CRLC UM Channel Establish REQ

LLA |  | RLC | @ 00:00:08.960

| BTS unit: |  | 1:1
| Channel No: |  | 1 Name: CCCH
| CFN: |  | 137

| Message Details:
| Configuration Parameters:
PU Size In Bits: | 152

#### CRLC UM Channel Establish CNF

RLC |  | LLA | @ 00:00:08.960

| BTS unit: |  | 1:1
| Channel No: |  | 1 Name: CCCH
| CFN: |  | 137

| Message Details:

#### CRLC_Config_CNF

LLA |  | RRC | @ 00:00:08.970

| Channel ID: |  | Rb0
| Cell ID: |  | 0

| Message Details:
| CRLC_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | 0

#### CRLC_Config_REQ

RRC |  | LLA | @ 00:00:08.970

| Channel ID: |  | Rb0
| Cell ID: |  | 0

| Message Details:
| CRLC_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | 0
ratType: | fdd
| configMessage: (CrlcConfigReq)
| setup: (RBInfo)
| sS_rlc_Info:
| sS_ul_RLC_Mode: (DL_RLC_Mode)
| dl_TM_RLC_Mode:
segmentationIndication: | false
| sS_dl_RLC_Mode:
dl_PayloadSize (PayloadSize): | 166
| dl_RLCModeInfo: (UL_RLC_Mode)
| ul_TM_RLC_Mode:
| transmissionRLC_Discard: Omit
segmentationIndication: | false
| rB_LogCH_Mapping:
uLlogicalChannelIdentity (LogicalChannelIdentity): | 5
dLlogicalChannelIdentity (LogicalChannelIdentity): | Omit
logicalChannelType: | Omit
cn_DomainIdentity: | Omit

#### CRLC TM Channel Establish REQ

LLA |  | RLC | @ 00:00:08.980

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: CCCH
| CFN: |  | 139

| Message Details:
| Configuration Parameters:
Number Of PU Sizes: | 1
| PU sizes In Bits:
Item 0: | 166

#### CRLC TM Channel Establish CNF

RLC |  | LLA | @ 00:00:08.980

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: CCCH
| CFN: |  | 139

| Message Details:

#### CRLC_Config_CNF

LLA |  | RRC | @ 00:00:08.990

| Channel ID: |  | Rb0
| Cell ID: |  | 0

| Message Details:
| CRLC_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | 0

#### CRLC_Config_REQ

RRC |  | LLA | @ 00:00:08.990

| Channel ID: |  | Rb1
| Cell ID: |  | -1

| Message Details:
| CRLC_Config_REQ:
cellId: | -1
| routingInfo:
rB_Identity: | 1
ratType: | fdd
| configMessage: (CrlcConfigReq)
| setup: (RBInfo)
| sS_rlc_Info:
| sS_ul_RLC_Mode: (DL_RLC_Mode)
dl_UM_RLC_Mode: |
| sS_dl_RLC_Mode:
dl_PayloadSize (PayloadSize): | 136
| dl_RLCModeInfo: (UL_RLC_Mode)
| ul_UM_RLC_Mode:
| transmissionRLC_Discard:
timerBasedNoExplicit (NoExplicitDiscard): | dt100
| rB_LogCH_Mapping:
uLlogicalChannelIdentity (LogicalChannelIdentity): | 1
dLlogicalChannelIdentity (LogicalChannelIdentity): | 1
logicalChannelType: | Omit
cn_DomainIdentity: | Omit

#### CRLC UM Channel Establish REQ

LLA |  | RLC | @ 00:00:08.990

| BTS unit: |  | 1:1
| Channel No: |  | 1 Name: DCCH
| CFN: |  | 140

| Message Details:
| Configuration Parameters:
PU Size In Bits: | 136

#### CRLC UM Channel Establish CNF

RLC |  | LLA | @ 00:00:08.990

| BTS unit: |  | 1:1
| Channel No: |  | 1 Name: DCCH
| CFN: |  | 140

| Message Details:

#### CRLC_Config_CNF

LLA |  | RRC | @ 00:00:09.000

| Channel ID: |  | Rb1
| Cell ID: |  | -1

| Message Details:
| CRLC_Config_CNF:
cellId: | -1
| routingInfo:
rB_Identity: | 1

#### CRLC_Config_REQ

RRC |  | LLA | @ 00:00:09.000

| Channel ID: |  | Rb2
| Cell ID: |  | -1

| Message Details:
| CRLC_Config_REQ:
cellId: | -1
| routingInfo:
rB_Identity: | 2
ratType: | fdd
| configMessage: (CrlcConfigReq)
| setup: (RBInfo)
| sS_rlc_Info:
| sS_ul_RLC_Mode: (DL_RLC_Mode)
| dl_AM_RLC_Mode:
inSequenceDelivery: | true
receivingWindowSize: | rw32
| dl_RLC_StatusInfo:
timerStatusProhibit: | tsp200
timerEPC: | Omit
missingPDU_Indicator: | true
timerStatusPeriodic: | Omit
| sS_dl_RLC_Mode:
dl_PayloadSize (PayloadSize): | 128
| dl_RLCModeInfo: (UL_RLC_Mode)
| ul_AM_RLC_Mode:
| transmissionRLC_Discard:
noDiscard (MaxDAT): | dat15
transmissionWindowSize: | tw32
timerRST: | tr500
max_RST (MaxRST): | rst1
| pollingInfo:
timerPollProhibit: | tpp200
timerPoll: | tp200
poll_PDU: | Omit
poll_SDU: | sdu1
lastTransmissionPDU_Poll: | true
lastRetransmissionPDU_Poll: | true
pollWindow: | pw99
timerPollPeriodic: | Omit
| rB_LogCH_Mapping:
uLlogicalChannelIdentity (LogicalChannelIdentity): | 2
dLlogicalChannelIdentity (LogicalChannelIdentity): | 2
logicalChannelType: | Omit
cn_DomainIdentity: | Omit

#### CRLC AM Channel Establish REQ

LLA |  | RLC | @ 00:00:09.010

| BTS unit: |  | 1:1
| Channel No: |  | 2 Name: DCCH
| CFN: |  | 142

| Message Details:
| Configuration Parameters:
PU Size In Bits: | 128
| Timer Parameters:
Poll (ms): | 200
Poll Prohibit (ms): | 0
EPC (ms): | 0
Discard (ms): | 0
Poll Periodic (ms): | 0
Status Prohibit (ms): | 0
Status Periodic (ms): | 0
Reset (ms): | 500
MRW (ms): | 0
| Protocol Parameters:
Max Dat: | 15
Poll PU: | 0
Poll SDU: | 1
Poll Window: | 99
Max Reset: | 1
Tx Window Size: | 32
Rx Window Size: | 32
Max MRW: | 0
SDU Discard Mode: | No discard
| Polling Triggers:
Last PU In Buffer: | On
Last PU In Retransmission Buffer: | On
Poll Timer: | On
Every Poll-PU PU: | Off
Every Poll-SDU SDU: | On
Poll-Window Percent Of Transmission Buffer: | On
Timer Based: | Off
| Status Triggers:
Missing PU: | On
Timer Based: | Off
EPC Mechanism: | Off

#### CRLC AM Channel Establish CNF

RLC |  | LLA | @ 00:00:09.010

| BTS unit: |  | 1:1
| Channel No: |  | 2 Name: DCCH
| CFN: |  | 142

| Message Details:

#### CRLC_Config_CNF

LLA |  | RRC | @ 00:00:09.020

| Channel ID: |  | Rb2
| Cell ID: |  | -1

| Message Details:
| CRLC_Config_CNF:
cellId: | -1
| routingInfo:
rB_Identity: | 2

#### CRLC_Config_REQ

RRC |  | LLA | @ 00:00:09.020

| Channel ID: |  | Rb3
| Cell ID: |  | -1

| Message Details:
| CRLC_Config_REQ:
cellId: | -1
| routingInfo:
rB_Identity: | 3
ratType: | fdd
| configMessage: (CrlcConfigReq)
| setup: (RBInfo)
| sS_rlc_Info:
| sS_ul_RLC_Mode: (DL_RLC_Mode)
| dl_AM_RLC_Mode:
inSequenceDelivery: | true
receivingWindowSize: | rw32
| dl_RLC_StatusInfo:
timerStatusProhibit: | tsp200
timerEPC: | Omit
missingPDU_Indicator: | true
timerStatusPeriodic: | Omit
| sS_dl_RLC_Mode:
dl_PayloadSize (PayloadSize): | 128
| dl_RLCModeInfo: (UL_RLC_Mode)
| ul_AM_RLC_Mode:
| transmissionRLC_Discard:
noDiscard (MaxDAT): | dat15
transmissionWindowSize: | tw32
timerRST: | tr500
max_RST (MaxRST): | rst1
| pollingInfo:
timerPollProhibit: | tpp200
timerPoll: | tp200
poll_PDU: | Omit
poll_SDU: | sdu1
lastTransmissionPDU_Poll: | true
lastRetransmissionPDU_Poll: | true
pollWindow: | pw99
timerPollPeriodic: | Omit
| rB_LogCH_Mapping:
uLlogicalChannelIdentity (LogicalChannelIdentity): | 3
dLlogicalChannelIdentity (LogicalChannelIdentity): | 3
logicalChannelType: | Omit
cn_DomainIdentity: | Omit

#### CRLC AM Channel Establish REQ

LLA |  | RLC | @ 00:00:09.020

| BTS unit: |  | 1:1
| Channel No: |  | 3 Name: DCCH
| CFN: |  | 143

| Message Details:
| Configuration Parameters:
PU Size In Bits: | 128
| Timer Parameters:
Poll (ms): | 200
Poll Prohibit (ms): | 0
EPC (ms): | 0
Discard (ms): | 0
Poll Periodic (ms): | 0
Status Prohibit (ms): | 0
Status Periodic (ms): | 0
Reset (ms): | 500
MRW (ms): | 0
| Protocol Parameters:
Max Dat: | 15
Poll PU: | 0
Poll SDU: | 1
Poll Window: | 99
Max Reset: | 1
Tx Window Size: | 32
Rx Window Size: | 32
Max MRW: | 0
SDU Discard Mode: | No discard
| Polling Triggers:
Last PU In Buffer: | On
Last PU In Retransmission Buffer: | On
Poll Timer: | On
Every Poll-PU PU: | Off
Every Poll-SDU SDU: | On
Poll-Window Percent Of Transmission Buffer: | On
Timer Based: | Off
| Status Triggers:
Missing PU: | On
Timer Based: | Off
EPC Mechanism: | Off

#### CRLC AM Channel Establish CNF

RLC |  | LLA | @ 00:00:09.020

| BTS unit: |  | 1:1
| Channel No: |  | 3 Name: DCCH
| CFN: |  | 143

| Message Details:

#### CRLC_Config_CNF

LLA |  | RRC | @ 00:00:09.040

| Channel ID: |  | Rb3
| Cell ID: |  | -1

| Message Details:
| CRLC_Config_CNF:
cellId: | -1
| routingInfo:
rB_Identity: | 3

#### CRLC_Config_REQ

RRC |  | LLA | @ 00:00:09.040

| Channel ID: |  | Rb4
| Cell ID: |  | -1

| Message Details:
| CRLC_Config_REQ:
cellId: | -1
| routingInfo:
rB_Identity: | 4
ratType: | fdd
| configMessage: (CrlcConfigReq)
| setup: (RBInfo)
| sS_rlc_Info:
| sS_ul_RLC_Mode: (DL_RLC_Mode)
| dl_AM_RLC_Mode:
inSequenceDelivery: | true
receivingWindowSize: | rw32
| dl_RLC_StatusInfo:
timerStatusProhibit: | tsp200
timerEPC: | Omit
missingPDU_Indicator: | true
timerStatusPeriodic: | Omit
| sS_dl_RLC_Mode:
dl_PayloadSize (PayloadSize): | 128
| dl_RLCModeInfo: (UL_RLC_Mode)
| ul_AM_RLC_Mode:
| transmissionRLC_Discard:
noDiscard (MaxDAT): | dat15
transmissionWindowSize: | tw32
timerRST: | tr500
max_RST (MaxRST): | rst1
| pollingInfo:
timerPollProhibit: | tpp200
timerPoll: | tp200
poll_PDU: | Omit
poll_SDU: | sdu1
lastTransmissionPDU_Poll: | true
lastRetransmissionPDU_Poll: | true
pollWindow: | pw99
timerPollPeriodic: | Omit
| rB_LogCH_Mapping:
uLlogicalChannelIdentity (LogicalChannelIdentity): | 4
dLlogicalChannelIdentity (LogicalChannelIdentity): | 4
logicalChannelType: | Omit
cn_DomainIdentity: | Omit

#### CRLC AM Channel Establish REQ

LLA |  | RLC | @ 00:00:09.040

| BTS unit: |  | 1:1
| Channel No: |  | 4 Name: DCCH
| CFN: |  | 145

| Message Details:
| Configuration Parameters:
PU Size In Bits: | 128
| Timer Parameters:
Poll (ms): | 200
Poll Prohibit (ms): | 0
EPC (ms): | 0
Discard (ms): | 0
Poll Periodic (ms): | 0
Status Prohibit (ms): | 0
Status Periodic (ms): | 0
Reset (ms): | 500
MRW (ms): | 0
| Protocol Parameters:
Max Dat: | 15
Poll PU: | 0
Poll SDU: | 1
Poll Window: | 99
Max Reset: | 1
Tx Window Size: | 32
Rx Window Size: | 32
Max MRW: | 0
SDU Discard Mode: | No discard
| Polling Triggers:
Last PU In Buffer: | On
Last PU In Retransmission Buffer: | On
Poll Timer: | On
Every Poll-PU PU: | Off
Every Poll-SDU SDU: | On
Poll-Window Percent Of Transmission Buffer: | On
Timer Based: | Off
| Status Triggers:
Missing PU: | On
Timer Based: | Off
EPC Mechanism: | Off

#### CRLC AM Channel Establish CNF

RLC |  | LLA | @ 00:00:09.040

| BTS unit: |  | 1:1
| Channel No: |  | 4 Name: DCCH
| CFN: |  | 145

| Message Details:

#### CRLC_Config_CNF

LLA |  | RRC | @ 00:00:09.050

| Channel ID: |  | Rb4
| Cell ID: |  | -1

| Message Details:
| CRLC_Config_CNF:
cellId: | -1
| routingInfo:
rB_Identity: | 4

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:09.050

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 27
bcch_ModificationTime: | Omit

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:09.070

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:09.070

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
noSegment: |

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA |  | RLC | @ 00:00:09.080

| Channel No: |  | 0 Name: BCCH

| Message Details:
| SIB repetition rate: 64
| SIB position: 54
| BCCH_BCH_Message:
| message:
| sfn_Prime: 0
| payload:
| noSegment: NULL
Layer 3 SDU: |
[0] | 00 | 00 |  |  |  |  |  |

#### o_SIB_PER_Encoding

RRC |  | RRC | @ 00:00:09.080

| Category: |  | TSO

| Message Details:
| Inputs:
| SIB:
| sIB1: (SysInfoType1)
cn_CommonGSM_MAP_NAS_SysInfo (NAS_SystemInformationGSM_MAP): |
[0] | 00 | 01 |  |  |  |  |  |
| cn_DomainSysInfoList:
| CN_DomainSysInfo:
cn_DomainIdentity: | ps_domain
| cn_Type:
gsm_MAP (NAS_SystemInformationGSM_MAP): |
[0] | 05 | 00 |  |  |  |  |  |
cn_DRX_CycleLengthCoeff (CN_DRX_CycleLengthCoefficient): | 7
| CN_DomainSysInfo:
cn_DomainIdentity: | cs_domain
| cn_Type:
gsm_MAP (NAS_SystemInformationGSM_MAP): |
[0] | 01 | 01 |  |  |  |  |  |
cn_DRX_CycleLengthCoeff (CN_DRX_CycleLengthCoefficient): | 7
| ue_ConnTimersAndConstants:
t_301: | Omit
n_301: | Omit
t_302: | Omit
n_302: | Omit
t_304: | Omit
n_304: | Omit
t_305: | Omit
t_307: | Omit
t_308: | Omit
t_309: | Omit
t_310: | Omit
n_310: | Omit
t_311: | Omit
t_312: | Omit
n_312: | Omit
t_313: | Omit
n_313: | Omit
t_314: | Omit
t_315: | Omit
n_315: | Omit
t_316: | Omit
t_317: | Omit
| ue_IdleTimersAndConstants:
t_300: | ms4000
n_300: | 3
t_312: | 10
n_312: | s1
| v3a0NonCriticalExtensions: Omit
| Outputs:
BITSTRING: |
[0] | 11 | 00 | 01 | 00 | 00 | 00 | 00 | 00
[8] | 00 | 00 | 01 | 01 | 10 | 00 | 10 | 00
[16] | 00 | 10 | 10 | 00 | 00 | 00 | 00 | 10
[24] | 00 | 01 | 00 | 00 | 00 | 01 | 00 | 00
[32] | 00 | 01 | 01 | 00 | 00 | 00 | 00 | 00
[40] | 00 | 00 | 00 | 00 | 00 | 00 | 11 | 00
[48] | 01 | 11 | 01 | 00 | 00 |  |  |

#### o_SIB_PER_Encoding

RRC |  | RRC | @ 00:00:09.080

| Category: |  | TSO

| Message Details:
| Inputs:
| SIB:
| sIB2: (SysInfoType2)
| ura_IdentityList:
URA_Identity: | 0000000000000001
| nonCriticalExtensions: Omit
| Outputs:
BITSTRING: |
[0] | 00 | 00 | 00 | 00 | 00 | 00 | 00 | 00
[8] | 00 | 01 |  |  |  |  |  |

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:09.080

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 11
bcch_ModificationTime: | Omit

#### MAC_DATA_REQ

RLC |  | MAC | @ 00:00:09.090

| Category: |  | Configuration
| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCCH
| CFN: |  | 150

| Message Details:
RLC PDU size (bits): | 16
RLC PDU (raw): |
[0] | 00 | 00 |  |  |  |  |  |

#### PHY_DATA_REQ

MAC |  | PHY | @ 00:00:09.090

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCH
| CFN: |  | 150

| Message Details:
SIB repetition period: | 64
SIB position: | 54
SIB size: | 246
SIB (raw): |
[0] | 00 | 00 | 00 | 00 | 00 | 00 | 00 | 00
[8] | 00 | 00 | 00 | 00 | 00 | 00 | 00 | 00
[16] | 00 | 00 | 00 | 00 | 00 | 00 | 00 | 00
[24] | 00 | 00 | 00 | 00 | 00 | 00 | 00 | 00
| SIB (decoded):
| TB 0:
MAC SDU (246 bits): |
[0] | 00 | 00 | 00 | 00 | 00 | 00 | 00 | 00
[8] | 00 | 00 | 00 | 00 | 00 | 00 | 00 | 00
[16] | 00 | 00 | 00 | 00 | 00 | 00 | 00 | 00
[24] | 00 | 00 | 00 | 00 | 00 | 00 | 00 |

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:09.100

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:09.100

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
| completeSIB_List:
| CompleteSIBshort:
sib_Type: | systemInformationBlockType1
sib_Data_variable: | 1100010000000000000001011000100000101000000000100001000000010000000101000000000000000000000011000111010000
| CompleteSIBshort:
sib_Type: | systemInformationBlockType2
sib_Data_variable: | 00000000000000000001

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA |  | RLC | @ 00:00:09.100

| Channel No: |  | 0 Name: BCCH

| Message Details:
| SIB repetition rate: 64
| SIB position: 22
| BCCH_BCH_Message:
| message:
| sfn_Prime: 0
| payload:
| completeSIB_List:
| CompleteSIB_List.element:
| sib_Type: systemInformationBlockType1_SIB_Type [enum=1]
| sib_Data_variable: 1100010000000000000001011000100000101000000000100001000000010000000101000000000000000000000011000111010000
| CompleteSIB_List.element:
| sib_Type: systemInformationBlockType2_SIB_Type [enum=2]
| sib_Data_variable: 00000000000000000001
Layer 3 SDU: |
[0] | 00 | 0E | 21 | 69 | C4 | 00 | 05 | 88
[8] | 28 | 02 | 10 | 10 | 14 | 00 | 00 | 0C
[16] | 74 | 04 | 26 | 00 | 00 | 20 |  |

#### o_SIB_PER_Encoding

RRC |  | RRC | @ 00:00:09.100

| Category: |  | TSO

| Message Details:
| Inputs:
| SIB:
| sIB2: (SysInfoType2)
| ura_IdentityList:
URA_Identity: | 0000000000000001
| nonCriticalExtensions: Omit
| Outputs:
BITSTRING: |
[0] | 00 | 00 | 00 | 00 | 00 | 00 | 00 | 00
[8] | 00 | 01 |  |  |  |  |  |

#### o_SIB_PER_Encoding

RRC |  | RRC | @ 00:00:09.100

| Category: |  | TSO

| Message Details:
| Inputs:
| SIB:
| sIB1: (SysInfoType1)
cn_CommonGSM_MAP_NAS_SysInfo (NAS_SystemInformationGSM_MAP): |
[0] | 00 | 01 |  |  |  |  |  |
| cn_DomainSysInfoList:
| CN_DomainSysInfo:
cn_DomainIdentity: | ps_domain
| cn_Type:
gsm_MAP (NAS_SystemInformationGSM_MAP): |
[0] | 05 | 00 |  |  |  |  |  |
cn_DRX_CycleLengthCoeff (CN_DRX_CycleLengthCoefficient): | 7
| CN_DomainSysInfo:
cn_DomainIdentity: | cs_domain
| cn_Type:
gsm_MAP (NAS_SystemInformationGSM_MAP): |
[0] | 01 | 01 |  |  |  |  |  |
cn_DRX_CycleLengthCoeff (CN_DRX_CycleLengthCoefficient): | 7
| ue_ConnTimersAndConstants:
t_301: | Omit
n_301: | Omit
t_302: | Omit
n_302: | Omit
t_304: | Omit
n_304: | Omit
t_305: | Omit
t_307: | Omit
t_308: | Omit
t_309: | Omit
t_310: | Omit
n_310: | Omit
t_311: | Omit
t_312: | Omit
n_312: | Omit
t_313: | Omit
n_313: | Omit
t_314: | Omit
t_315: | Omit
n_315: | Omit
t_316: | Omit
t_317: | Omit
| ue_IdleTimersAndConstants:
t_300: | ms4000
n_300: | 3
t_312: | 10
n_312: | s1
| v3a0NonCriticalExtensions: Omit
| Outputs:
BITSTRING: |
[0] | 11 | 00 | 01 | 00 | 00 | 00 | 00 | 00
[8] | 00 | 00 | 01 | 01 | 10 | 00 | 10 | 00
[16] | 00 | 10 | 10 | 00 | 00 | 00 | 00 | 10
[24] | 00 | 01 | 00 | 00 | 00 | 01 | 00 | 00
[32] | 00 | 01 | 01 | 00 | 00 | 00 | 00 | 00
[40] | 00 | 00 | 00 | 00 | 00 | 00 | 11 | 00
[48] | 01 | 11 | 01 | 00 | 00 |  |  |

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:09.100

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 11
bcch_ModificationTime: | Omit

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:09.110

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:09.110

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
| completeSIB_List:
| CompleteSIBshort:
sib_Type: | systemInformationBlockType1
sib_Data_variable: | 1100010000000000000001011000100000101000000000100001000000010000000101000000000000000000000011000111010000
| CompleteSIBshort:
sib_Type: | systemInformationBlockType2
sib_Data_variable: | 00000000000000000001

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA |  | RLC | @ 00:00:09.110

| Channel No: |  | 0 Name: BCCH

| Message Details:
| SIB repetition rate: 64
| SIB position: 22
| BCCH_BCH_Message:
| message:
| sfn_Prime: 0
| payload:
| completeSIB_List:
| CompleteSIB_List.element:
| sib_Type: systemInformationBlockType1_SIB_Type [enum=1]
| sib_Data_variable: 1100010000000000000001011000100000101000000000100001000000010000000101000000000000000000000011000111010000
| CompleteSIB_List.element:
| sib_Type: systemInformationBlockType2_SIB_Type [enum=2]
| sib_Data_variable: 00000000000000000001
Layer 3 SDU: |
[0] | 00 | 0E | 21 | 69 | C4 | 00 | 05 | 88
[8] | 28 | 02 | 10 | 10 | 14 | 00 | 00 | 0C
[16] | 74 | 04 | 26 | 00 | 00 | 20 |  |

#### o_SIB_PER_Encoding

RRC |  | RRC | @ 00:00:09.110

| Category: |  | TSO

| Message Details:
| Inputs:
| SIB:
| sIB3: (SysInfoType3)
sib4indicator: | true
cellIdentity: | 0000000000000000000000000000
| cellSelectReselectInfo: (CellSelectReselectInfoSIB_3_4)
| mappingInfo: Omit
| cellSelectQualityMeasure:
cpich_RSCP: |
| modeSpecificInfo:
| fdd:
s_Intrasearch (S_SearchQual): | 8
s_Intersearch (S_SearchQual): | 8
s_SearchHCS (S_SearchRXLEV): | Omit
| rat_List: (RAT_FDD_InfoList)
| RAT_FDD_Info:
rat_Identifier: | gsm
s_SearchRAT (S_SearchQual): | -16
s_HCS_RAT (S_SearchRXLEV): | Omit
s_Limit_SearchRAT (S_SearchQual): | 0
q_QualMin: | -24
q_RxlevMin: | -40
q_Hyst_l_S (Q_Hyst_S): | 2
t_Reselection_S: | 0
| hcs_ServingCellInformation: Omit
maxAllowedUL_TX_Power: | 21
| cellAccessRestriction:
| cellBarred:
notBarred: |
cellReservedForOperatorUse (ReservedIndicator): | notReserved
cellReservationExtension (ReservedIndicator): | notReserved
| accessClassBarredList:
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
| nonCriticalExtensions: Omit
| Outputs:
BITSTRING: |
[0] | 01 | 00 | 00 | 00 | 00 | 00 | 00 | 00
[8] | 00 | 00 | 00 | 00 | 00 | 00 | 00 | 00
[16] | 10 | 11 | 01 | 11 | 00 | 01 | 10 | 00
[24] | 00 | 00 | 00 | 00 | 00 | 01 | 00 | 00
[32] | 00 | 00 | 00 | 10 | 01 | 00 | 00 | 10
[40] | 00 | 00 | 01 | 00 | 01 | 11 | 11 | 11
[48] | 11 | 11 | 11 | 11 | 11 | 11 | 11 | 11

#### o_SIB_PER_Encoding

RRC |  | RRC | @ 00:00:09.110

| Category: |  | TSO

| Message Details:
| Inputs:
| SIB:
| sIB7: (SysInfoType7)
| modeSpecificInfo:
| fdd:
ul_Interference: | -100
| prach_Information_SIB5_List: (DynamicPersistenceLevelList)
DynamicPersistenceLevel: | 2
| prach_Information_SIB6_List: (DynamicPersistenceLevelList)
DynamicPersistenceLevel: | 2
expirationTimeFactor: | Omit
| nonCriticalExtensions: Omit
| Outputs:
BITSTRING: |
[0] | 10 | 00 | 00 | 10 | 10 | 00 | 00 | 00
[8] | 10 | 00 | 00 | 01 |  |  |  |

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:09.110

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 10
bcch_ModificationTime: | Omit

#### MAC_DATA_REQ

RLC |  | MAC | @ 00:00:09.110

| Category: |  | Configuration
| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCCH
| CFN: |  | 152

| Message Details:
RLC PDU size (bits): | 176
RLC PDU (raw): |
[0] | 00 | 0E | 21 | 69 | C4 | 00 | 05 | 88
[8] | 28 | 02 | 10 | 10 | 14 | 00 | 00 | 0C
[16] | 74 | 04 | 26 | 00 | 00 | 20 |  |

#### PHY_DATA_REQ

MAC |  | PHY | @ 00:00:09.110

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCH
| CFN: |  | 152

| Message Details:
SIB repetition period: | 64
SIB position: | 22
SIB size: | 246
SIB (raw): |
[0] | 00 | 0E | 21 | 69 | C4 | 00 | 05 | 88
[8] | 28 | 02 | 10 | 10 | 14 | 00 | 00 | 0C
[16] | 74 | 04 | 26 | 00 | 00 | 20 | 00 | 00
[24] | 00 | 00 | 00 | 00 | 00 | 00 | 00 | 00
| SIB (decoded):
| TB 0:
MAC SDU (246 bits): |
[0] | 00 | 0E | 21 | 69 | C4 | 00 | 05 | 88
[8] | 28 | 02 | 10 | 10 | 14 | 00 | 00 | 0C
[16] | 74 | 04 | 26 | 00 | 00 | 20 | 00 | 00
[24] | 00 | 00 | 00 | 00 | 00 | 00 | 00 |

#### MAC_DATA_REQ

RLC |  | MAC | @ 00:00:09.120

| Category: |  | Configuration
| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCCH
| CFN: |  | 153

| Message Details:
RLC PDU size (bits): | 176
RLC PDU (raw): |
[0] | 00 | 0E | 21 | 69 | C4 | 00 | 05 | 88
[8] | 28 | 02 | 10 | 10 | 14 | 00 | 00 | 0C
[16] | 74 | 04 | 26 | 00 | 00 | 20 |  |

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:09.130

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:09.130

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
| completeSIB_List:
| CompleteSIBshort:
sib_Type: | systemInformationBlockType7
sib_Data_variable: | 100000101000000010000001
| CompleteSIBshort:
sib_Type: | systemInformationBlockType3
sib_Data_variable: | 0100000000000000000000000000000010110111000110000000000000010000000000100100001000000100011111111111111111111111

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA |  | RLC | @ 00:00:09.130

| Channel No: |  | 0 Name: BCCH

| Message Details:
| SIB repetition rate: 64
| SIB position: 20
| BCCH_BCH_Message:
| message:
| sfn_Prime: 0
| payload:
| completeSIB_List:
| CompleteSIB_List.element:
| sib_Type: systemInformationBlockType7_SIB_Type [enum=7]
| sib_Data_variable: 100000101000000010000001
| CompleteSIB_List.element:
| sib_Type: systemInformationBlockType3_SIB_Type [enum=3]
| sib_Data_variable: 0100000000000000000000000000000010110111000110000000000000010000000000100100001000000100011111111111111111111111
Layer 3 SDU: |
[0] | 00 | 0E | 27 | 17 | 82 | 80 | 81 | 1B
[8] | 7A | 00 | 00 | 00 | 05 | B8 | C0 | 00
[16] | 80 | 12 | 10 | 23 | FF | FF | F8 |

#### o_SIB_PER_Encoding

RRC |  | RRC | @ 00:00:09.130

| Category: |  | TSO

| Message Details:
| Inputs:
| SIB:
| sIB4: (SysInfoType4)
cellIdentity: | 0000000000000000000000000000
| cellSelectReselectInfo: (CellSelectReselectInfoSIB_3_4)
| mappingInfo: Omit
| cellSelectQualityMeasure:
cpich_RSCP: |
| modeSpecificInfo:
| fdd:
s_Intrasearch (S_SearchQual): | 8
s_Intersearch (S_SearchQual): | 8
s_SearchHCS (S_SearchRXLEV): | Omit
| rat_List: (RAT_FDD_InfoList)
| RAT_FDD_Info:
rat_Identifier: | gsm
s_SearchRAT (S_SearchQual): | -16
s_HCS_RAT (S_SearchRXLEV): | Omit
s_Limit_SearchRAT (S_SearchQual): | 0
q_QualMin: | -24
q_RxlevMin: | -40
q_Hyst_l_S (Q_Hyst_S): | 0
t_Reselection_S: | 0
| hcs_ServingCellInformation: Omit
maxAllowedUL_TX_Power: | 21
| cellAccessRestriction:
| cellBarred:
notBarred: |
cellReservedForOperatorUse (ReservedIndicator): | notReserved
cellReservationExtension (ReservedIndicator): | notReserved
| accessClassBarredList: Omit
| nonCriticalExtensions: Omit
| Outputs:
BITSTRING: |
[0] | 00 | 00 | 00 | 00 | 00 | 00 | 00 | 00
[8] | 00 | 00 | 00 | 00 | 00 | 00 | 00 | 01
[16] | 01 | 10 | 11 | 10 | 00 | 11 | 00 | 00
[24] | 00 | 00 | 00 | 00 | 00 | 10 | 00 | 00
[32] | 00 | 00 | 01 | 00 | 10 | 00 | 00 | 00
[40] | 00 | 00 | 10 | 00 | 11 | 10 | 11 | 1

#### PHY_DATA_REQ

MAC |  | PHY | @ 00:00:09.130

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCH
| CFN: |  | 154

| Message Details:
SIB repetition period: | 64
SIB position: | 22
SIB size: | 246
SIB (raw): |
[0] | 00 | 0E | 21 | 69 | C4 | 00 | 05 | 88
[8] | 28 | 02 | 10 | 10 | 14 | 00 | 00 | 0C
[16] | 74 | 04 | 26 | 00 | 00 | 20 | 00 | 00
[24] | 00 | 00 | 00 | 00 | 00 | 00 | 00 | 00
| SIB (decoded):
| TB 0:
MAC SDU (246 bits): |
[0] | 00 | 0E | 21 | 69 | C4 | 00 | 05 | 88
[8] | 28 | 02 | 10 | 10 | 14 | 00 | 00 | 0C
[16] | 74 | 04 | 26 | 00 | 00 | 20 | 00 | 00
[24] | 00 | 00 | 00 | 00 | 00 | 00 | 00 |

#### o_SIB_PER_Encoding

RRC |  | RRC | @ 00:00:09.140

| Category: |  | TSO

| Message Details:
| Inputs:
| SIB:
| sIB7: (SysInfoType7)
| modeSpecificInfo:
| fdd:
ul_Interference: | -100
| prach_Information_SIB5_List: (DynamicPersistenceLevelList)
DynamicPersistenceLevel: | 2
| prach_Information_SIB6_List: (DynamicPersistenceLevelList)
DynamicPersistenceLevel: | 2
expirationTimeFactor: | Omit
| nonCriticalExtensions: Omit
| Outputs:
BITSTRING: |
[0] | 10 | 00 | 00 | 10 | 10 | 00 | 00 | 00
[8] | 10 | 00 | 00 | 01 |  |  |  |

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:09.140

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 26
bcch_ModificationTime: | Omit

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:09.160

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:09.160

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
| completeSIB_List:
| CompleteSIBshort:
sib_Type: | systemInformationBlockType7
sib_Data_variable: | 100000101000000010000001
| CompleteSIBshort:
sib_Type: | systemInformationBlockType4
sib_Data_variable: | 00000000000000000000000000000001011011100011000000000000001000000000010010000000000010001110111

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA |  | RLC | @ 00:00:09.160

| Channel No: |  | 0 Name: BCCH

| Message Details:
| SIB repetition rate: 64
| SIB position: 52
| BCCH_BCH_Message:
| message:
| sfn_Prime: 0
| payload:
| completeSIB_List:
| CompleteSIB_List.element:
| sib_Type: systemInformationBlockType7_SIB_Type [enum=7]
| sib_Data_variable: 100000101000000010000001
| CompleteSIB_List.element:
| sib_Type: systemInformationBlockType4_SIB_Type [enum=4]
| sib_Data_variable: 00000000000000000000000000000001011011100011000000000000001000000000010010000000000010001110111
Layer 3 SDU: |
[0] | 00 | 0E | 27 | 17 | 82 | 80 | 81 | 22
[8] | F0 | 00 | 00 | 00 | 0B | 71 | 80 | 01
[16] | 00 | 24 | 00 | 47 | 70 |  |  |

#### o_SIB_PER_Encoding

RRC |  | RRC | @ 00:00:09.180

| Category: |  | TSO

| Message Details:
| Inputs:
| SIB:
| sIB5: (SysInfoType5)
sib6indicator: | true
pich_PowerOffset: | -5
| modeSpecificInfo:
| fdd:
aich_PowerOffset: | -5
| primaryCCPCH_Info: Omit
| prach_SystemInformationList:
| PRACH_SystemInformation:
| prach_RACH_Info:
| modeSpecificInfo:
| fdd:
availableSignatures: | 0000000011111111
availableSF (SF_PRACH): | sfpr64
preambleScramblingCodeWordNumber: | 0
puncturingLimit: | pl1
availableSubChannelNumbers: | 111111111111
transportChannelIdentity: | 15
| rach_TransportFormatSet: (TransportFormatSet)
| commonTransChTFS:
| tti:
| tti20: (CommonDynamicTF_InfoList)
| CommonDynamicTF_Info:
| rlc_Size:
| fdd:
| octetModeRLC_SizeInfoType2:
sizeType1: | 15
| numberOfTbSizeList:
| NumberOfTransportBlocks:
one: |
| logicalChannelList:
configured: |
| CommonDynamicTF_Info:
| rlc_Size:
| fdd:
| octetModeRLC_SizeInfoType2:
sizeType2: | 3
| numberOfTbSizeList:
| NumberOfTransportBlocks:
one: |
| logicalChannelList:
configured: |
| semistaticTF_Information:
| channelCodingType:
convolutional (CodingRate): | half
rateMatchingAttribute: | 150
crc_Size: | crc16
| rach_TFCS: (TFCS)
| normalTFCI_Signalling: (ExplicitTFCS_Configuration)
| complete: (TFCS_ReconfAdd)
| ctfcSize:
| ctfc2Bit:
| :
ctfc2: | 0
| powerOffsetInformation:
| gainFactorInformation:
computedGainFactors (ReferenceTFC_ID): | 0
powerOffsetPp_m: | 0
| :
ctfc2: | 1
| powerOffsetInformation:
| gainFactorInformation:
| signalledGainFactors:
| modeSpecificInfo:
| fdd:
gainFactorBetaC (GainFactor): | 11
gainFactorBetaD (GainFactor): | 15
referenceTFC_ID: | 0
powerOffsetPp_m: | 0
| prach_Partitioning:
| fdd:
| ASCSetting_FDD:
| accessServiceClass_FDD: Omit
| ASCSetting_FDD:
| accessServiceClass_FDD:
availableSignatureStartIndex: | 0
availableSignatureEndIndex: | 7
assignedSubChannelNumber: | 1111
| ASCSetting_FDD:
| accessServiceClass_FDD: Omit
| ASCSetting_FDD:
| accessServiceClass_FDD:
availableSignatureStartIndex: | 0
availableSignatureEndIndex: | 7
assignedSubChannelNumber: | 1111
| ASCSetting_FDD:
| accessServiceClass_FDD: Omit
| ASCSetting_FDD:
| accessServiceClass_FDD:
availableSignatureStartIndex: | 0
availableSignatureEndIndex: | 7
assignedSubChannelNumber: | 1111
| ASCSetting_FDD:
| accessServiceClass_FDD: Omit
| ASCSetting_FDD:
| accessServiceClass_FDD:
availableSignatureStartIndex: | 0
availableSignatureEndIndex: | 7
assignedSubChannelNumber: | 1111
| persistenceScalingFactorList:
PersistenceScalingFactor: | psf0_9
PersistenceScalingFactor: | psf0_9
PersistenceScalingFactor: | psf0_9
PersistenceScalingFactor: | psf0_9
PersistenceScalingFactor: | psf0_9
PersistenceScalingFactor: | psf0_9
| ac_To_ASC_MappingTable:
AC_To_ASC_Mapping: | 6
AC_To_ASC_Mapping: | 5
AC_To_ASC_Mapping: | 4
AC_To_ASC_Mapping: | 3
AC_To_ASC_Mapping: | 2
AC_To_ASC_Mapping: | 1
AC_To_ASC_Mapping: | 0
| modeSpecificInfo:
| fdd:
primaryCPICH_TX_Power: | 31
constantValue: | -10
| prach_PowerOffset:
powerRampStep: | 3
preambleRetransMax: | 4
| rach_TransmissionParameters:
mmax: | 2
nb01Min (NB01): | 3
nb01Max (NB01): | 10
| aich_Info:
channelisationCode256: | 3
sttd_Indicator: | false
aich_TransmissionTiming: | e0
| sCCPCH_SystemInformationList:
| SCCPCH_SystemInformation:
| secondaryCCPCH_Info:
| modeSpecificInfo:
| fdd:
dummy1 (PCPICH_UsageForChannelEst): | mayBeUsed
| dummy2: (SecondaryCPICH_Info) Omit
secondaryScramblingCode: | Omit
sttd_Indicator: | false
| sf_AndCodeNumber: (SF256_AndCodeNumber)
sf64: | 1
pilotSymbolExistence: | false
tfci_Existence: | true
positionFixedOrFlexible: | flexible
timingOffset: | 0
| tfcs:
| normalTFCI_Signalling: (ExplicitTFCS_Configuration)
| complete: (TFCS_ReconfAdd)
| ctfcSize:
| ctfc4Bit:
| :
ctfc4: | 0
| powerOffsetInformation: Omit
| :
ctfc4: | 1
| powerOffsetInformation: Omit
| :
ctfc4: | 2
| powerOffsetInformation: Omit
| :
ctfc4: | 3
| powerOffsetInformation: Omit
| :
ctfc4: | 4
| powerOffsetInformation: Omit
| :
ctfc4: | 5
| powerOffsetInformation: Omit
| :
ctfc4: | 6
| powerOffsetInformation: Omit
| :
ctfc4: | 8
| powerOffsetInformation: Omit
| fach_PCH_InformationList:
| FACH_PCH_Information:
| transportFormatSet:
| commonTransChTFS:
| tti:
| tti10: (CommonDynamicTF_InfoList)
| CommonDynamicTF_Info:
| rlc_Size:
| fdd:
| octetModeRLC_SizeInfoType2:
sizeType1: | 24
| numberOfTbSizeList:
| NumberOfTransportBlocks:
zero: |
| NumberOfTransportBlocks:
one: |
| logicalChannelList:
allSizes: |
| semistaticTF_Information:
| channelCodingType:
convolutional (CodingRate): | half
rateMatchingAttribute: | 230
crc_Size: | crc16
transportChannelIdentity: | 12
ctch_Indicator: | false
| FACH_PCH_Information:
| transportFormatSet:
| commonTransChTFS:
| tti:
| tti10: (CommonDynamicTF_InfoList)
| CommonDynamicTF_Info:
| rlc_Size:
| fdd:
| octetModeRLC_SizeInfoType2:
sizeType1: | 15
| numberOfTbSizeList:
| NumberOfTransportBlocks:
zero: |
| NumberOfTransportBlocks:
one: |
| NumberOfTransportBlocks:
small: | 2
| logicalChannelList:
allSizes: |
| semistaticTF_Information:
| channelCodingType:
convolutional (CodingRate): | half
rateMatchingAttribute: | 220
crc_Size: | crc16
transportChannelIdentity: | 13
ctch_Indicator: | false
| FACH_PCH_Information:
| transportFormatSet:
| commonTransChTFS:
| tti:
| tti10: (CommonDynamicTF_InfoList)
| CommonDynamicTF_Info:
| rlc_Size:
| fdd:
| octetModeRLC_SizeInfoType2:
sizeType2: | 3
| numberOfTbSizeList:
| NumberOfTransportBlocks:
zero: |
| NumberOfTransportBlocks:
one: |
| logicalChannelList:
allSizes: |
| semistaticTF_Information:
| channelCodingType:
turbo: |
rateMatchingAttribute: | 130
crc_Size: | crc16
transportChannelIdentity: | 14
ctch_Indicator: | false
| pich_Info:
| fdd:
channelisationCode256: | 2
pi_CountPerFrame: | e18
sttd_Indicator: | false
| cbs_DRX_Level1Information: Omit
| nonCriticalExtensions: Omit
| Outputs:
BITSTRING: |
[0] | 00 | 01 | 01 | 01 | 01 | 00 | 01 | 00
[8] | 00 | 11 | 11 | 10 | 00 | 00 | 00 | 00
[16] | 11 | 11 | 11 | 11 | 01 | 00 | 00 | 11
[24] | 11 | 11 | 11 | 11 | 11 | 11 | 11 | 01
[32] | 11 | 01 | 00 | 10 | 00 | 01 | 00 | 00
[40] | 11 | 11 | 00 | 00 | 00 | 10 | 10 | 01
[48] | 00 | 00 | 11 | 00 | 00 | 00 | 10 | 10
[56] | 10 | 10 | 01 | 01 | 01 | 01 | 10 | 00
[64] | 00 | 00 | 00 | 00 | 00 | 00 | 11 | 00
[72] | 11 | 00 | 01 | 01 | 10 | 11 | 01 | 01
[80] | 01 | 11 | 11 | 10 | 00 | 10 | 10 | 11
[88] | 10 | 10 | 00 | 00 | 11 | 11 | 11 | 10
[96] | 10 | 00 | 00 | 11 | 11 | 11 | 10 | 10
[104] | 00 | 00 | 11 | 11 | 11 | 10 | 10 | 00
[112] | 00 | 11 | 11 | 11 | 11 | 01 | 00 | 00
[120] | 00 | 00 | 00 | 00 | 00 | 00 | 00 | 11
[128] | 01 | 01 | 10 | 00 | 11 | 01 | 00 | 01
[136] | 00 | 00 | 11 | 11 | 11 | 01 | 00 | 11
[144] | 10 | 01 | 01 | 00 | 00 | 01 | 10 | 00
[152] | 01 | 00 | 00 | 11 | 00 | 10 | 10 | 00
[160] | 00 | 00 | 11 | 00 | 00 | 00 | 11 | 10
[168] | 00 | 00 | 01 | 00 | 00 | 00 | 01 | 01
[176] | 10 | 00 | 00 | 10 | 00 | 00 | 00 | 11
[184] | 10 | 00 | 00 | 00 | 00 | 10 | 00 | 10
[192] | 00 | 01 | 10 | 01 | 00 | 00 | 10 | 10
[200] | 01 | 10 | 01 | 00 | 00 | 10 | 10 | 00
[208] | 00 | 00 | 00 | 00 | 11 | 00 | 00 | 00
[216] | 01 | 00 | 01 | 00 | 01 | 01 | 11 | 00
[224] | 10 | 10 | 11 | 01 | 01 | 10 | 10 | 00
[232] | 00 | 00 | 00 | 00 | 01 | 11 | 10 | 00
[240] | 10 | 00 | 01 | 10 | 00 | 00 | 00 | 01
[248] | 01 | 10 | 11 | 01 | 10 | 11 | 01 | 10
[256] | 00 | 10 | 00 | 00 | 00 | 00 | 01 | 00
[264] | 00 | 11 | 00 | 00 | 10 | 00 | 10 | 01
[272] | 01 | 00 | 00 | 00 | 10 | 11 | 01 | 10
[280] | 10 | 00 | 00 | 00 | 01 | 00 | 00 |

#### MAC_DATA_REQ

RLC |  | MAC | @ 00:00:09.190

| Category: |  | Configuration
| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCCH
| CFN: |  | 160

| Message Details:
RLC PDU size (bits): | 184
RLC PDU (raw): |
[0] | 00 | 0E | 27 | 17 | 82 | 80 | 81 | 1B
[8] | 7A | 00 | 00 | 00 | 05 | B8 | C0 | 00
[16] | 80 | 12 | 10 | 23 | FF | FF | F8 |

#### MAC_DATA_REQ

RLC |  | MAC | @ 00:00:09.190

| Category: |  | Configuration
| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCCH
| CFN: |  | 160

| Message Details:
RLC PDU size (bits): | 168
RLC PDU (raw): |
[0] | 00 | 0E | 27 | 17 | 82 | 80 | 81 | 22
[8] | F0 | 00 | 00 | 00 | 0B | 71 | 80 | 01
[16] | 00 | 24 | 00 | 47 | 70 |  |  |

#### PHY_DATA_REQ

MAC |  | PHY | @ 00:00:09.190

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCH
| CFN: |  | 160

| Message Details:
SIB repetition period: | 64
SIB position: | 20
SIB size: | 246
SIB (raw): |
[0] | 00 | 0E | 27 | 17 | 82 | 80 | 81 | 1B
[8] | 7A | 00 | 00 | 00 | 05 | B8 | C0 | 00
[16] | 80 | 12 | 10 | 23 | FF | FF | F8 | 00
[24] | 00 | 00 | 00 | 00 | 00 | 00 | 00 | 00
| SIB (decoded):
| TB 0:
MAC SDU (246 bits): |
[0] | 00 | 0E | 27 | 17 | 82 | 80 | 81 | 1B
[8] | 7A | 00 | 00 | 00 | 05 | B8 | C0 | 00
[16] | 80 | 12 | 10 | 23 | FF | FF | F8 | 00
[24] | 00 | 00 | 00 | 00 | 00 | 00 | 00 |

#### PHY_DATA_REQ

MAC |  | PHY | @ 00:00:09.210

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCH
| CFN: |  | 162

| Message Details:
SIB repetition period: | 64
SIB position: | 52
SIB size: | 246
SIB (raw): |
[0] | 00 | 0E | 27 | 17 | 82 | 80 | 81 | 22
[8] | F0 | 00 | 00 | 00 | 0B | 71 | 80 | 01
[16] | 00 | 24 | 00 | 47 | 70 | FF | F8 | 00
[24] | 00 | 00 | 00 | 00 | 00 | 00 | 00 | 00
| SIB (decoded):
| TB 0:
MAC SDU (246 bits): |
[0] | 00 | 0E | 27 | 17 | 82 | 80 | 81 | 22
[8] | F0 | 00 | 00 | 00 | 0B | 71 | 80 | 01
[16] | 00 | 24 | 00 | 47 | 70 | FF | F8 | 00
[24] | 00 | 00 | 00 | 00 | 00 | 00 | 00 |

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:09.220

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 23
bcch_ModificationTime: | Omit

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:09.240

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:09.240

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
noSegment: |

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA |  | RLC | @ 00:00:09.240

| Channel No: |  | 0 Name: BCCH

| Message Details:
| SIB repetition rate: 64
| SIB position: 46
| BCCH_BCH_Message:
| message:
| sfn_Prime: 0
| payload:
| noSegment: NULL
Layer 3 SDU: |
[0] | 00 | 00 |  |  |  |  |  |

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:09.240

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 19
bcch_ModificationTime: | Omit

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:09.250

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:09.250

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
| firstSegment:
sib_Type: | systemInformationBlockType5
seg_Count (SegCount): | 3
sib_Data_fixed: | 000101010100010000111110000000001111111101000011111111111111110111010010000100001111000000101001000011000000101010100101010110000000000000001100110001011011010101111110001010111010000011111110100000111111101000001111111010

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA |  | RLC | @ 00:00:09.250

| Channel No: |  | 0 Name: BCCH

| Message Details:
| SIB repetition rate: 64
| SIB position: 38
| BCCH_BCH_Message:
| message:
| sfn_Prime: 0
| payload:
| firstSegment:
| sib_Type: systemInformationBlockType5_SIB_Type [enum=5]
| seg_Count: 3
| sib_Data_fixed: 000101010100010000111110000000001111111101000011111111111111110111010010000100001111000000101001000011000000101010100101010110000000000000001100110001011011010101111110001010111010000011111110100000111111101000001111111010
Layer 3 SDU: |
[0] | 00 | 02 | 52 | 15 | 44 | 3E | 00 | FF
[8] | 43 | FF | FD | D2 | 10 | F0 | 29 | 0C
[16] | 0A | A5 | 58 | 00 | 0C | C5 | B5 | 7E
[24] | 2B | A0 | FE | 83 | FA | 0F | E8 |

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:09.250

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 21
bcch_ModificationTime: | Omit

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:09.270

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:09.270

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
| subsequentSegment:
sib_Type: | systemInformationBlockType5
segmentIndex: | 1
sib_Data_fixed: | 000011111111010000000000000000001101011000110100010000111111010011100101000001100001000011001010000000110000001110000001000000010110000010000000111000000000100010000110010000101001100100001010000000000011000000010001000101

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA |  | RLC | @ 00:00:09.270

| Channel No: |  | 0 Name: BCCH

| Message Details:
| SIB repetition rate: 64
| SIB position: 42
| BCCH_BCH_Message:
| message:
| sfn_Prime: 0
| payload:
| subsequentSegment:
| sib_Type: systemInformationBlockType5_SIB_Type [enum=5]
| segmentIndex: 1
| sib_Data_fixed: 000011111111010000000000000000001101011000110100010000111111010011100101000001100001000011001010000000110000001110000001000000010110000010000000111000000000100010000110010000101001100100001010000000000011000000010001000101
Layer 3 SDU: |
[0] | 00 | 04 | 50 | 0F | F4 | 00 | 00 | D6
[8] | 34 | 43 | F4 | E5 | 06 | 10 | CA | 03
[16] | 03 | 81 | 01 | 60 | 80 | E0 | 08 | 86
[24] | 42 | 99 | 0A | 00 | 30 | 11 | 14 |

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:09.270

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 22
bcch_ModificationTime: | Omit

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:09.290

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:09.290

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
| lastSegmentShort:
sib_Type: | systemInformationBlockType5
segmentIndex: | 2
sib_Data_variable: | 1100101011010110100000000000011110001000011000000001011011011011011000100000000001000011000010001001010000001011011010000000010000

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA |  | RLC | @ 00:00:09.290

| Channel No: |  | 0 Name: BCCH

| Message Details:
| SIB repetition rate: 64
| SIB position: 44
| BCCH_BCH_Message:
| message:
| sfn_Prime: 0
| payload:
| lastSegmentShort:
| sib_Type: systemInformationBlockType5_SIB_Type [enum=5]
| segmentIndex: 2
| sib_Data_variable: 1100101011010110100000000000011110001000011000000001011011011011011000100000000001000011000010001001010000001011011010000000010000
Layer 3 SDU: |
[0] | 00 | 06 | 51 | 81 | CA | D6 | 80 | 07
[8] | 88 | 60 | 16 | DB | 62 | 00 | 43 | 08
[16] | 94 | 0B | 68 | 04 | 00 |  |  |

#### o_SIB_PER_Encoding

RRC |  | RRC | @ 00:00:09.290

| Category: |  | TSO

| Message Details:
| Inputs:
| SIB:
| sIB6: (SysInfoType6)
pich_PowerOffset: | -5
| modeSpecificInfo:
| fdd:
aich_PowerOffset: | -5
dummy (CSICH_PowerOffset): | Omit
| primaryCCPCH_Info: Omit
| prach_SystemInformationList: Omit
| sCCPCH_SystemInformationList: Omit
| cbs_DRX_Level1Information: Omit
| nonCriticalExtensions: Omit
| Outputs:
BITSTRING: |
[0] | 00 | 00 | 00 | 10 | 10 | 01 | 00 | 01

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:09.290

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 3
bcch_ModificationTime: | Omit

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:09.300

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:09.300

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
| completeSIB_List:
| CompleteSIBshort:
sib_Type: | systemInformationBlockType6
sib_Data_variable: | 0000001010010001

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA |  | RLC | @ 00:00:09.300

| Channel No: |  | 0 Name: BCCH

| Message Details:
| SIB repetition rate: 64
| SIB position: 6
| BCCH_BCH_Message:
| message:
| sfn_Prime: 0
| payload:
| completeSIB_List:
| CompleteSIB_List.element:
| sib_Type: systemInformationBlockType6_SIB_Type [enum=6]
| sib_Data_variable: 0000001010010001
Layer 3 SDU: |
[0] | 00 | 0E | 06 | 0F | 02 | 91 |  |

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:09.300

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 5
bcch_ModificationTime: | Omit

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:09.320

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:09.320

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
noSegment: |

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA |  | RLC | @ 00:00:09.320

| Channel No: |  | 0 Name: BCCH

| Message Details:
| SIB repetition rate: 64
| SIB position: 10
| BCCH_BCH_Message:
| message:
| sfn_Prime: 0
| payload:
| noSegment: NULL
Layer 3 SDU: |
[0] | 00 | 00 |  |  |  |  |  |

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:09.320

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 6
bcch_ModificationTime: | Omit

#### MAC_DATA_REQ

RLC |  | MAC | @ 00:00:09.320

| Category: |  | Configuration
| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCCH
| CFN: |  | 173

| Message Details:
RLC PDU size (bits): | 16
RLC PDU (raw): |
[0] | 00 | 00 |  |  |  |  |  |

#### MAC_DATA_REQ

RLC |  | MAC | @ 00:00:09.320

| Category: |  | Configuration
| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCCH
| CFN: |  | 173

| Message Details:
RLC PDU size (bits): | 248
RLC PDU (raw): |
[0] | 00 | 02 | 52 | 15 | 44 | 3E | 00 | FF
[8] | 43 | FF | FD | D2 | 10 | F0 | 29 | 0C
[16] | 0A | A5 | 58 | 00 | 0C | C5 | B5 | 7E
[24] | 2B | A0 | FE | 83 | FA | 0F | E8 |

#### MAC_DATA_REQ

RLC |  | MAC | @ 00:00:09.320

| Category: |  | Configuration
| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCCH
| CFN: |  | 173

| Message Details:
RLC PDU size (bits): | 248
RLC PDU (raw): |
[0] | 00 | 04 | 50 | 0F | F4 | 00 | 00 | D6
[8] | 34 | 43 | F4 | E5 | 06 | 10 | CA | 03
[16] | 03 | 81 | 01 | 60 | 80 | E0 | 08 | 86
[24] | 42 | 99 | 0A | 00 | 30 | 11 | 14 |

#### MAC_DATA_REQ

RLC |  | MAC | @ 00:00:09.320

| Category: |  | Configuration
| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCCH
| CFN: |  | 173

| Message Details:
RLC PDU size (bits): | 168
RLC PDU (raw): |
[0] | 00 | 06 | 51 | 81 | CA | D6 | 80 | 07
[8] | 88 | 60 | 16 | DB | 62 | 00 | 43 | 08
[16] | 94 | 0B | 68 | 04 | 00 |  |  |

#### MAC_DATA_REQ

RLC |  | MAC | @ 00:00:09.320

| Category: |  | Configuration
| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCCH
| CFN: |  | 173

| Message Details:
RLC PDU size (bits): | 48
RLC PDU (raw): |
[0] | 00 | 0E | 06 | 0F | 02 | 91 |  |

#### MAC_DATA_REQ

RLC |  | MAC | @ 00:00:09.320

| Category: |  | Configuration
| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCCH
| CFN: |  | 173

| Message Details:
RLC PDU size (bits): | 16
RLC PDU (raw): |
[0] | 00 | 00 |  |  |  |  |  |

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:09.330

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:09.330

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
noSegment: |

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA |  | RLC | @ 00:00:09.330

| Channel No: |  | 0 Name: BCCH

| Message Details:
| SIB repetition rate: 64
| SIB position: 12
| BCCH_BCH_Message:
| message:
| sfn_Prime: 0
| payload:
| noSegment: NULL
Layer 3 SDU: |
[0] | 00 | 00 |  |  |  |  |  |

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:09.330

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 7
bcch_ModificationTime: | Omit

#### PHY_DATA_REQ

MAC |  | PHY | @ 00:00:09.330

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCH
| CFN: |  | 174

| Message Details:
SIB repetition period: | 64
SIB position: | 46
SIB size: | 246
SIB (raw): |
[0] | 00 | 00 | 27 | 17 | 82 | 80 | 81 | 22
[8] | F0 | 00 | 00 | 00 | 0B | 71 | 80 | 01
[16] | 00 | 24 | 00 | 47 | 70 | FF | F8 | 00
[24] | 00 | 00 | 00 | 00 | 00 | 00 | 00 | 00
| SIB (decoded):
| TB 0:
MAC SDU (246 bits): |
[0] | 00 | 00 | 27 | 17 | 82 | 80 | 81 | 22
[8] | F0 | 00 | 00 | 00 | 0B | 71 | 80 | 01
[16] | 00 | 24 | 00 | 47 | 70 | FF | F8 | 00
[24] | 00 | 00 | 00 | 00 | 00 | 00 | 00 |

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:09.350

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:09.350

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
noSegment: |

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA |  | RLC | @ 00:00:09.350

| Channel No: |  | 0 Name: BCCH

| Message Details:
| SIB repetition rate: 64
| SIB position: 14
| BCCH_BCH_Message:
| message:
| sfn_Prime: 0
| payload:
| noSegment: NULL
Layer 3 SDU: |
[0] | 00 | 00 |  |  |  |  |  |

#### o_SIB_PER_Encoding

RRC |  | RRC | @ 00:00:09.350

| Category: |  | TSO

| Message Details:
| Inputs:
| SIB:
| sIB7: (SysInfoType7)
| modeSpecificInfo:
| fdd:
ul_Interference: | -100
| prach_Information_SIB5_List: (DynamicPersistenceLevelList)
DynamicPersistenceLevel: | 2
| prach_Information_SIB6_List: (DynamicPersistenceLevelList)
DynamicPersistenceLevel: | 2
expirationTimeFactor: | Omit
| nonCriticalExtensions: Omit
| Outputs:
BITSTRING: |
[0] | 10 | 00 | 00 | 10 | 10 | 00 | 00 | 00
[8] | 10 | 00 | 00 | 01 |  |  |  |

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:09.350

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 2
bcch_ModificationTime: | Omit

#### MAC_DATA_REQ

RLC |  | MAC | @ 00:00:09.350

| Category: |  | Configuration
| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCCH
| CFN: |  | 176

| Message Details:
RLC PDU size (bits): | 16
RLC PDU (raw): |
[0] | 00 | 00 |  |  |  |  |  |

#### MAC_DATA_REQ

RLC |  | MAC | @ 00:00:09.350

| Category: |  | Configuration
| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCCH
| CFN: |  | 176

| Message Details:
RLC PDU size (bits): | 16
RLC PDU (raw): |
[0] | 00 | 00 |  |  |  |  |  |

#### PHY_DATA_REQ

MAC |  | PHY | @ 00:00:09.350

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCH
| CFN: |  | 176

| Message Details:
SIB repetition period: | 64
SIB position: | 38
SIB size: | 246
SIB (raw): |
[0] | 00 | 02 | 52 | 15 | 44 | 3E | 00 | FF
[8] | 43 | FF | FD | D2 | 10 | F0 | 29 | 0C
[16] | 0A | A5 | 58 | 00 | 0C | C5 | B5 | 7E
[24] | 2B | A0 | FE | 83 | FA | 0F | E8 | 00
| SIB (decoded):
| TB 0:
MAC SDU (246 bits): |
[0] | 00 | 02 | 52 | 15 | 44 | 3E | 00 | FF
[8] | 43 | FF | FD | D2 | 10 | F0 | 29 | 0C
[16] | 0A | A5 | 58 | 00 | 0C | C5 | B5 | 7E
[24] | 2B | A0 | FE | 83 | FA | 0F | E8 |

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:09.360

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:09.360

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
| completeSIB_List:
| CompleteSIBshort:
sib_Type: | systemInformationBlockType7
sib_Data_variable: | 100000101000000010000001

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA |  | RLC | @ 00:00:09.360

| Channel No: |  | 0 Name: BCCH

| Message Details:
| SIB repetition rate: 64
| SIB position: 4
| BCCH_BCH_Message:
| message:
| sfn_Prime: 0
| payload:
| completeSIB_List:
| CompleteSIB_List.element:
| sib_Type: systemInformationBlockType7_SIB_Type [enum=7]
| sib_Data_variable: 100000101000000010000001
Layer 3 SDU: |
[0] | 00 | 0E | 07 | 17 | 82 | 80 | 81 |

#### o_SIB_PER_Encoding

RRC |  | RRC | @ 00:00:09.360

| Category: |  | TSO

| Message Details:
| Inputs:
| SIB:
| sIB7: (SysInfoType7)
| modeSpecificInfo:
| fdd:
ul_Interference: | -100
| prach_Information_SIB5_List: (DynamicPersistenceLevelList)
DynamicPersistenceLevel: | 2
| prach_Information_SIB6_List: (DynamicPersistenceLevelList)
DynamicPersistenceLevel: | 2
expirationTimeFactor: | Omit
| nonCriticalExtensions: Omit
| Outputs:
BITSTRING: |
[0] | 10 | 00 | 00 | 10 | 10 | 00 | 00 | 00
[8] | 10 | 00 | 00 | 01 |  |  |  |

#### o_SIB_PER_Encoding

RRC |  | RRC | @ 00:00:09.360

| Category: |  | TSO

| Message Details:
| Inputs:
| SIB:
| sIB3: (SysInfoType3)
sib4indicator: | true
cellIdentity: | 0000000000000000000000000000
| cellSelectReselectInfo: (CellSelectReselectInfoSIB_3_4)
| mappingInfo: Omit
| cellSelectQualityMeasure:
cpich_RSCP: |
| modeSpecificInfo:
| fdd:
s_Intrasearch (S_SearchQual): | 8
s_Intersearch (S_SearchQual): | 8
s_SearchHCS (S_SearchRXLEV): | Omit
| rat_List: (RAT_FDD_InfoList)
| RAT_FDD_Info:
rat_Identifier: | gsm
s_SearchRAT (S_SearchQual): | -16
s_HCS_RAT (S_SearchRXLEV): | Omit
s_Limit_SearchRAT (S_SearchQual): | 0
q_QualMin: | -24
q_RxlevMin: | -40
q_Hyst_l_S (Q_Hyst_S): | 2
t_Reselection_S: | 0
| hcs_ServingCellInformation: Omit
maxAllowedUL_TX_Power: | 21
| cellAccessRestriction:
| cellBarred:
notBarred: |
cellReservedForOperatorUse (ReservedIndicator): | notReserved
cellReservationExtension (ReservedIndicator): | notReserved
| accessClassBarredList:
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
| nonCriticalExtensions: Omit
| Outputs:
BITSTRING: |
[0] | 01 | 00 | 00 | 00 | 00 | 00 | 00 | 00
[8] | 00 | 00 | 00 | 00 | 00 | 00 | 00 | 00
[16] | 10 | 11 | 01 | 11 | 00 | 01 | 10 | 00
[24] | 00 | 00 | 00 | 00 | 00 | 01 | 00 | 00
[32] | 00 | 00 | 00 | 10 | 01 | 00 | 00 | 10
[40] | 00 | 00 | 01 | 00 | 01 | 11 | 11 | 11
[48] | 11 | 11 | 11 | 11 | 11 | 11 | 11 | 11

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:09.360

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 10
bcch_ModificationTime: | Omit

#### PHY_DATA_REQ

MAC |  | PHY | @ 00:00:09.370

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCH
| CFN: |  | 178

| Message Details:
SIB repetition period: | 64
SIB position: | 42
SIB size: | 246
SIB (raw): |
[0] | 00 | 04 | 50 | 0F | F4 | 00 | 00 | D6
[8] | 34 | 43 | F4 | E5 | 06 | 10 | CA | 03
[16] | 03 | 81 | 01 | 60 | 80 | E0 | 08 | 86
[24] | 42 | 99 | 0A | 00 | 30 | 11 | 14 | 00
| SIB (decoded):
| TB 0:
MAC SDU (246 bits): |
[0] | 00 | 04 | 50 | 0F | F4 | 00 | 00 | D6
[8] | 34 | 43 | F4 | E5 | 06 | 10 | CA | 03
[16] | 03 | 81 | 01 | 60 | 80 | E0 | 08 | 86
[24] | 42 | 99 | 0A | 00 | 30 | 11 | 14 |

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:09.380

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:09.380

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
| completeSIB_List:
| CompleteSIBshort:
sib_Type: | systemInformationBlockType7
sib_Data_variable: | 100000101000000010000001
| CompleteSIBshort:
sib_Type: | systemInformationBlockType3
sib_Data_variable: | 0100000000000000000000000000000010110111000110000000000000010000000000100100001000000100011111111111111111111111

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA |  | RLC | @ 00:00:09.380

| Channel No: |  | 0 Name: BCCH

| Message Details:
| SIB repetition rate: 64
| SIB position: 20
| BCCH_BCH_Message:
| message:
| sfn_Prime: 0
| payload:
| completeSIB_List:
| CompleteSIB_List.element:
| sib_Type: systemInformationBlockType7_SIB_Type [enum=7]
| sib_Data_variable: 100000101000000010000001
| CompleteSIB_List.element:
| sib_Type: systemInformationBlockType3_SIB_Type [enum=3]
| sib_Data_variable: 0100000000000000000000000000000010110111000110000000000000010000000000100100001000000100011111111111111111111111
Layer 3 SDU: |
[0] | 00 | 0E | 27 | 17 | 82 | 80 | 81 | 1B
[8] | 7A | 00 | 00 | 00 | 05 | B8 | C0 | 00
[16] | 80 | 12 | 10 | 23 | FF | FF | F8 |

#### o_SIB_PER_Encoding

RRC |  | RRC | @ 00:00:09.380

| Category: |  | TSO

| Message Details:
| Inputs:
| SIB:
| sIB18: (SysInfoType18)
| idleModePLMNIdentities: (PLMNIdentitiesOfNeighbourCells)
| plmnsOfIntraFreqCellsList: Omit
| plmnsOfInterFreqCellsList: Omit
| plmnsOfInterRATCellsList: Omit
| connectedModePLMNIdentities: (PLMNIdentitiesOfNeighbourCells) Omit
| nonCriticalExtensions: Omit
| Outputs:
BITSTRING: |
[0] | 10 | 00 | 00 |  |  |  |  |

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:09.380

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 18
bcch_ModificationTime: | Omit

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:09.390

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:09.390

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
| completeSIB_List:
| CompleteSIBshort:
sib_Type:
| systemInformationBlockType7
sib_Data_variable: | 100000101000000010000001
| CompleteSIBshort:
sib_Type: | systemInformationBlockType18
sib_Data_variable: | 100000

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA |  | RLC | @ 00:00:09.390

| Channel No: |  | 0 Name: BCCH

| Message Details:
| SIB repetition rate: 64
| SIB position: 36
| BCCH_BCH_Message:
| message:
| sfn_Prime: 0
| payload:
| completeSIB_List:
| CompleteSIB_List.element:
| sib_Type: systemInformationBlockType7_SIB_Type [enum=7]
| sib_Data_variable: 100000101000000010000001
| CompleteSIB_List.element:
| sib_Type: systemInformationBlockType18_SIB_Type [enum=26]
| sib_Data_variable: 100000
Layer 3 SDU: |
[0] | 00 | 0E | 27 | 17 | 82 | 80 | 81 | D0
[8] | 2C | 00 |  |  |  |  |  |

#### o_SIB_PER_Encoding

RRC |  | RRC | @ 00:00:09.390

| Category: |  | TSO

| Message Details:
| Inputs:
| SIB:
| sIB4: (SysInfoType4)
cellIdentity: | 0000000000000000000000000000
| cellSelectReselectInfo: (CellSelectReselectInfoSIB_3_4)
| mappingInfo: Omit
| cellSelectQualityMeasure:
cpich_RSCP: |
| modeSpecificInfo:
| fdd:
s_Intrasearch (S_SearchQual): | 8
s_Intersearch (S_SearchQual): | 8
s_SearchHCS (S_SearchRXLEV): | Omit
| rat_List: (RAT_FDD_InfoList)
| RAT_FDD_Info:
rat_Identifier: | gsm
s_SearchRAT (S_SearchQual): | -16
s_HCS_RAT (S_SearchRXLEV): | Omit
s_Limit_SearchRAT (S_SearchQual): | 0
q_QualMin: | -24
q_RxlevMin: | -40
q_Hyst_l_S (Q_Hyst_S): | 0
t_Reselection_S: | 0
| hcs_ServingCellInformation: Omit
maxAllowedUL_TX_Power: | 21
| cellAccessRestriction:
| cellBarred:
notBarred: |
cellReservedForOperatorUse (ReservedIndicator): | notReserved
cellReservationExtension (ReservedIndicator): | notReserved
| accessClassBarredList: Omit
| nonCriticalExtensions: Omit

| Outputs:
BITSTRING: |
[0] | 00 | 00 | 00 | 00 | 00 | 00 | 00 | 00
[8] | 00 | 00 | 00 | 00 | 00 | 00 | 00 | 01
[16] | 01 | 10 | 11 | 10 | 00 | 11 | 00 | 00
[24] | 00 | 00 | 00 | 00 | 00 | 10 | 00 | 00
[32] | 00 | 00 | 01 | 00 | 10 | 00 | 00 | 00
[40] | 00 | 00 | 10 | 00 | 11 | 10 | 11 | 1

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:09.390

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 26
bcch_ModificationTime: | Omit

#### PHY_DATA_REQ

MAC |  | PHY | @ 00:00:09.390

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCH
| CFN: |  | 180

| Message Details:
SIB repetition period: | 64
SIB position: | 44
SIB size: | 246
SIB (raw): |
[0] | 00 | 06 | 51 | 81 | CA | D6 | 80 | 07
[8] | 88 | 60 | 16 | DB | 62 | 00 | 43 | 08
[16] | 94 | 0B | 68 | 04 | 00 | E0 | 08 | 86
[24] | 42 | 99 | 0A | 00 | 30 | 11 | 14 | 00
| SIB (decoded):
| TB 0:
MAC SDU (246 bits): |
[0] | 00 | 06 | 51 | 81 | CA | D6 | 80 | 07
[8] | 88 | 60 | 16 | DB | 62 | 00 | 43 | 08
[16] | 94 | 0B | 68 | 04 | 00 | E0 | 08 | 86
[24] | 42 | 99 | 0A | 00 | 30 | 11 | 14 |

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:09.410

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:09.410

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
| completeSIB_List:
| CompleteSIBshort:
sib_Type:
| systemInformationBlockType7
sib_Data_variable: | 100000101000000010000001
| CompleteSIBshort:
sib_Type: | systemInformationBlockType4
sib_Data_variable: | 00000000000000000000000000000001011011100011000000000000001000000000010010000000000010001110111

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA |  | RLC | @ 00:00:09.410

| Channel No: |  | 0 Name: BCCH

| Message Details:
| SIB repetition rate: 64
| SIB position: 52
| BCCH_BCH_Message:
| message:
| sfn_Prime: 0
| payload:
| completeSIB_List:
| CompleteSIB_List.element:
| sib_Type: systemInformationBlockType7_SIB_Type [enum=7]
| sib_Data_variable: 100000101000000010000001
| CompleteSIB_List.element:
| sib_Type: systemInformationBlockType4_SIB_Type [enum=4]
| sib_Data_variable: 00000000000000000000000000000001011011100011000000000000001000000000010010000000000010001110111

Layer 3 SDU: |
[0] | 00 | 0E | 27 | 17 | 82 | 80 | 81 | 22
[8] | F0 | 00 | 00 | 00 | 0B | 71 | 80 | 01
[16] | 00 | 24 | 00 | 47 | 70 |  |  |

#### o_SIB_PER_Encoding

RRC |  | RRC | @ 00:00:09.410

| Category: |  | TSO

| Message Details:
| Inputs:
| SIB:
| sIB11: (SysInfoType11)
sib12indicator: | true
| fach_MeasurementOccasionInfo: Omit
| measurementControlSysInfo:
| use_of_HCS:
| hcs_not_used:
| cellSelectQualityMeasure:
| cpich_RSCP:
| intraFreqMeasurementSysInfo: (IntraFreqMeasurementSysInfo_RSCP)
intraFreqMeasurementID (MeasurementIdentity): | Omit
| intraFreqCellInfoSI_List: (IntraFreqCellInfoSI_List_RSCP)
| removedIntraFreqCellList: Omit
| newIntraFreqCellList: (NewIntraFreqCellSI_List_RSCP)
| NewIntraFreqCellSI_RSCP:
intraFreqCellID: | 0
| cellInfo: (CellInfoSI_RSCP)
cellIndividualOffset: | Omit
| referenceTimeDifferenceToCell: Omit
| modeSpecificInfo:
| fdd:
| primaryCPICH_Info:
primaryScramblingCode: | 100
primaryCPICH_TX_Power: | Omit
readSFN_Indicator: | false
tx_DiversityIndicator: | false
| cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP) Omit

| NewIntraFreqCellSI_RSCP:
intraFreqCellID: | 1
| cellInfo: (CellInfoSI_RSCP)
cellIndividualOffset: | Omit
| referenceTimeDifferenceToCell: Omit
| modeSpecificInfo:
| fdd:
| primaryCPICH_Info:
primaryScramblingCode: | 150
primaryCPICH_TX_Power: | Omit
readSFN_Indicator: | true
tx_DiversityIndicator: | false
| cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP) Omit

| NewIntraFreqCellSI_RSCP:
intraFreqCellID: | 2
| cellInfo: (CellInfoSI_RSCP)
cellIndividualOffset: | Omit
| referenceTimeDifferenceToCell: Omit
| modeSpecificInfo:
| fdd:
| primaryCPICH_Info:
primaryScramblingCode:
| 200
primaryCPICH_TX_Power: | Omit
readSFN_Indicator: | true
tx_DiversityIndicator: | false
| cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP) Omit

| NewIntraFreqCellSI_RSCP:
intraFreqCellID: | 6
| cellInfo: (CellInfoSI_RSCP)
cellIndividualOffset: | Omit
| referenceTimeDifferenceToCell: Omit
| modeSpecificInfo:
| fdd:
| primaryCPICH_Info:
primaryScramblingCode:
| 400
primaryCPICH_TX_Power: | Omit
readSFN_Indicator: | true
tx_DiversityIndicator: | false
| cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP) Omit

| NewIntraFreqCellSI_RSCP:
intraFreqCellID: | 7
| cellInfo: (CellInfoSI_RSCP)
cellIndividualOffset: | Omit
| referenceTimeDifferenceToCell: Omit
| modeSpecificInfo:
| fdd:
| primaryCPICH_Info:
primaryScramblingCode:
| 450
primaryCPICH_TX_Power: | Omit
readSFN_Indicator: | true
tx_DiversityIndicator: | false
| cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP) Omit

| intraFreqMeasQuantity:
filterCoefficient: | Omit
| modeSpecificInfo:
| fdd:
intraFreqMeasQuantity_FDD: | cpich_RSCP

| intraFreqReportingQuantityForRACH: Omit

maxReportedCellsOnRACH: | Omit

| reportingInfoForCellDCH:
| intraFreqReportingQuantity:
| activeSetReportingQuantities: (CellReportingQuantities)
dummy (SFN_SFN_OTD_Type): | noReport
cellIdentity_reportingIndicator: | true
cellSynchronisationInfoReportingIndicator: | false
| modeSpecificInfo:
| fdd:
cpich_Ec_N0_reportingIndicator:
| false
cpich_RSCP_reportingIndicator: | true
pathloss_reportingIndicator: | false
| monitoredSetReportingQuantities: (CellReportingQuantities)
dummy (SFN_SFN_OTD_Type): | noReport
cellIdentity_reportingIndicator: | true
cellSynchronisationInfoReportingIndicator: | true
| modeSpecificInfo:
| fdd:
cpich_Ec_N0_reportingIndicator: | false
cpich_RSCP_reportingIndicator: | true
pathloss_reportingIndicator: | false
| detectedSetReportingQuantities: (CellReportingQuantities) Omit

| measurementReportingMode:
measurementReportTransferMode (TransferMode): | acknowledgedModeRLC
periodicalOrEventTrigger: | eventTrigger

| reportCriteria: (CellDCH_ReportCriteria)
| intraFreqReportingCriteria:
| eventCriteriaList: (IntraFreqEventCriteriaList)
| IntraFreqEventCriteria:
| event: (IntraFreqEvent)
| e1a: (Event1a)
triggeringCondition (TriggeringCondition2):
| monitoredSetCellsOnly
reportingRange: | 5
| forbiddenAffectCellList: Omit
w: | 1
reportDeactivationThreshold: | t2
reportingAmount: | ra4
reportingInterval: | ri4
hysteresis: | 0
timeToTrigger: | ttt640
| reportingCellStatus:
withinActiveAndOrMonitoredUsedFreq (MaxNumberOfReportingCellsType1): | e3
| IntraFreqEventCriteria:
| event: (IntraFreqEvent)
| e1b: (Event1b)
triggeringCondition (TriggeringCondition1): | activeSetCellsOnly
reportingRange: | 5
| forbiddenAffectCellList: Omit
w: | 1
hysteresis: | 0
timeToTrigger: | ttt640
| reportingCellStatus:
withinActiveAndOrMonitoredUsedFreq (MaxNumberOfReportingCellsType1): | e3
| IntraFreqEventCriteria:
| event: (IntraFreqEvent)
| e1c: (Event1c)
replacementActivationThreshold: | t3
reportingAmount: | ra4
reportingInterval: | ri4
hysteresis: | 0
timeToTrigger: | ttt640
| reportingCellStatus:
withinActiveAndOrMonitoredUsedFreq (MaxNumberOfReportingCellsType1): | e3

| interFreqMeasurementSysInfo: (InterFreqMeasurementSysInfo_RSCP)
| interFreqCellInfoSI_List: (InterFreqCellInfoSI_List_RSCP)
| removedInterFreqCellList: Omit
| newInterFreqCellList: (NewInterFreqCellSI_List_RSCP)
| NewInterFreqCellSI_RSCP:
interFreqCellID: | 3
| frequencyInfo:
| modeSpecificInfo:
| fdd: (FrequencyInfoFDD)
uarfcn_UL (UARFCN):
| Omit
uarfcn_DL (UARFCN): | 10837
| cellInfo: (CellInfoSI_RSCP)
cellIndividualOffset: | Omit
| referenceTimeDifferenceToCell: Omit
| modeSpecificInfo:
| fdd:
| primaryCPICH_Info:
primaryScramblingCode:
| 250
primaryCPICH_TX_Power: | Omit
readSFN_Indicator: | false
tx_DiversityIndicator: | false
| cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP) Omit

| NewInterFreqCellSI_RSCP:
interFreqCellID: | 4
| frequencyInfo: Omit
| cellInfo: (CellInfoSI_RSCP)
cellIndividualOffset: | Omit
| referenceTimeDifferenceToCell: Omit
| modeSpecificInfo:
| fdd:
| primaryCPICH_Info:
primaryScramblingCode:
| 300
primaryCPICH_TX_Power: | Omit
readSFN_Indicator: | false
tx_DiversityIndicator: | false
| cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP) Omit

| NewInterFreqCellSI_RSCP:
interFreqCellID: | 5
| frequencyInfo: Omit
| cellInfo: (CellInfoSI_RSCP)
cellIndividualOffset: | Omit
| referenceTimeDifferenceToCell: Omit
| modeSpecificInfo:
| fdd:
| primaryCPICH_Info:
primaryScramblingCode:
| 350
primaryCPICH_TX_Power: | Omit
readSFN_Indicator: | false
tx_DiversityIndicator: | false
| cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP) Omit

| interRATMeasurementSysInfo: (InterRATMeasurementSysInfo_B) Omit

| trafficVolumeMeasSysInfo: Omit

| dummy: (UE_InternalMeasurementSysInfo) Omit

| nonCriticalExtensions: Omit

| Outputs:
BITSTRING: |
[0] | 00 | 10 | 00 | 00 | 11 | 01 | 10 | 01
[8] | 00 | 01 | 00 | 10 | 00 | 00 | 00 | 00
[16] | 10 | 00 | 11 | 00 | 10 | 00 | 01 | 00
[24] | 00 | 10 | 00 | 01 | 00 | 10 | 01 | 01
[32] | 10 | 10 | 10 | 00 | 10 | 00 | 00 | 10
[40] | 01 | 10 | 01 | 00 | 01 | 01 | 00 | 11
[48] | 00 | 00 | 01 | 01 | 10 | 01 | 00 | 00
[56] | 10 | 10 | 01 | 11 | 00 | 00 | 10 | 11
[64] | 10 | 00 | 01 | 01 | 00 | 00 | 10 | 00
[72] | 10 | 00 | 10 | 00 | 11 | 00 | 10 | 01
[80] | 01 | 01 | 01 | 00 | 00 | 00 | 01 | 00
[88] | 10 | 10 | 00 | 01 | 01 | 00 | 10 | 10
[96] | 10 | 00 | 01 | 10 | 00 | 01 | 00 | 10
[104] | 10 | 00 | 10 | 00 | 00 | 10 | 10 | 00
[112] | 01 | 00 | 00 | 11 | 00 | 00 | 10 | 01
[120] | 01 | 00 | 10 | 01 | 10 | 10 | 10 | 10
[128] | 00 | 01 | 10 | 00 | 01 | 00 | 10 | 10
[136] | 10 | 00 | 10 | 11 | 00 | 01 | 10 | 01
[144] | 01 | 01 | 00 | 10 | 10 | 10 | 10 | 00
[152] | 01 | 00 | 11 | 11 | 10 | 10 | 00 | 10
[160] | 00 | 10 | 00 | 00 | 01 | 01 | 00 | 10
[168] | 11 | 00 | 00 | 10 | 00 | 10 | 10 | 00
[176] | 01 | 01 | 01 | 01 | 11 | 10 | 00 |

#### PHY_DATA_REQ

MAC |  | PHY | @ 00:00:09.410

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCH
| CFN: |  | 182

| Message Details:
SIB repetition period: | 64
SIB position: | 6
SIB size: | 246
SIB (raw): |
[0] | 00 | 0E | 06 | 0F | 02 | 91 | 80 | 07
[8] | 88 | 60 | 16 | DB | 62 | 00 | 43 | 08
[16] | 94 | 0B | 68 | 04 | 00 | E0 | 08 | 86
[24] | 42 | 99 | 0A | 00 | 30 | 11 | 14 | 00
| SIB (decoded):
| TB 0:
MAC SDU (246 bits): |
[0] | 00 | 0E | 06 | 0F | 02 | 91 | 80 | 07
[8] | 88 | 60 | 16 | DB | 62 | 00 | 43 | 08
[16] | 94 | 0B | 68 | 04 | 00 | E0 | 08 | 86
[24] | 42 | 99 | 0A | 00 | 30 | 11 | 14 |

#### PHY_DATA_REQ

MAC |  | PHY | @ 00:00:09.430

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCH
| CFN: |  | 184

| Message Details:
SIB repetition period: | 64
SIB position: | 10
SIB size: | 246
SIB (raw): |
[0] | 00 | 00 | 06 | 0F | 02 | 91 | 80 | 07
[8] | 88 | 60 | 16 | DB | 62 | 00 | 43 | 08
[16] | 94 | 0B | 68 | 04 | 00 | E0 | 08 | 86
[24] | 42 | 99 | 0A | 00 | 30 | 11 | 14 | 00
| SIB (decoded):
| TB 0:
MAC SDU (246 bits): |
[0] | 00 | 00 | 06 | 0F | 02 | 91 | 80 | 07
[8] | 88 | 60 | 16 | DB | 62 | 00 | 43 | 08
[16] | 94 | 0B | 68 | 04 | 00 | E0 | 08 | 86
[24] | 42 | 99 | 0A | 00 | 30 | 11 | 14 |

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:09.440

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 31
bcch_ModificationTime: | Omit

#### PHY_DATA_REQ

MAC |  | PHY | @ 00:00:09.450

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCH
| CFN: |  | 186

| Message Details:
SIB repetition period: | 64
SIB position: | 12
SIB size: | 246
SIB (raw): |
[0] | 00 | 00 | 06 | 0F | 02 | 91 | 80 | 07
[8] | 88 | 60 | 16 | DB | 62 | 00 | 43 | 08
[16] | 94 | 0B | 68 | 04 | 00 | E0 | 08 | 86
[24] | 42 | 99 | 0A | 00 | 30 | 11 | 14 | 00
| SIB (decoded):
| TB 0:
MAC SDU (246 bits): |
[0]
| 00 | 00 | 06 | 0F | 02 | 91 | 80 | 07
[8] | 88 | 60 | 16 | DB | 62 | 00 | 43 | 08
[16] | 94 | 0B | 68 | 04 | 00 | E0 | 08 | 86
[24] | 42 | 99 | 0A | 00 | 30 | 11 | 14 |

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:09.460

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:09.460

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
noSegment: |

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA |  | RLC | @ 00:00:09.460

| Channel No: |  | 0 Name: BCCH

| Message Details:
| SIB repetition rate: 64
| SIB position: 62
| BCCH_BCH_Message:
| message:
| sfn_Prime: 0
| payload:
| noSegment: NULL

Layer 3 SDU: |
[0] | 00 | 00 |  |  |  |  |  |

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:09.460

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 29
bcch_ModificationTime: | Omit

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:09.470

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:09.470

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId:
| 0
| routingInfo:
rB_Identity:
| -1

| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
| firstSegment:
sib_Type: | systemInformationBlockType11
seg_Count (SegCount): | 2
sib_Data_fixed: | 001000001101100100010010000000001000110010000100001000010010010110101000100000100110010001010011000001011001000010100111000010111000010100001000100010001100100101010100000001001010000101001010100001100001001010001000001010

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA |  | RLC | @ 00:00:09.470

| Channel No: |  | 0 Name: BCCH

| Message Details:
| SIB repetition rate: 64
| SIB position: 58
| BCCH_BCH_Message:
| message:
| sfn_Prime: 0
| payload:
| firstSegment:
| sib_Type: systemInformationBlockType11_SIB_Type [enum=11]
| seg_Count: 2
| sib_Data_fixed: 001000001101100100010010000000001000110010000100001000010010010110101000100000100110010001010011000001011001000010100111000010111000010100001000100010001100100101010100000001001010000101001010100001100001001010001000001010

Layer 3 SDU: |
[0] | 00 | 02 | B1 | 20 | D9 | 12 | 00 | 8C
[8] | 84 | 21 | 25 | A8 | 82 | 64 | 53 | 05
[16] | 90 | A7 | 0B | 85 | 08 | 88 | C9 | 54
[24] | 04 | A1 | 4A | 86 | 12 | 88 | 28 |

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:09.470

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1

ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 30
bcch_ModificationTime: | Omit

#### PHY_DATA_REQ

MAC |  | PHY | @ 00:00:09.470

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCH
| CFN: |  | 188

| Message Details:
SIB repetition period:
| 64
SIB position: | 14
SIB size: | 246
SIB (raw): |
[0]
| 00 | 00 | 06 | 0F | 02 | 91 | 80 | 07
[8] | 88 | 60 | 16 | DB | 62 | 00 | 43 | 08
[16] | 94 | 0B | 68 | 04 | 00 | E0 | 08 | 86
[24] | 42 | 99 | 0A | 00 | 30 | 11 | 14 | 00

| SIB (decoded):
| TB 0:
MAC SDU (246 bits): |
[0] | 00 | 00 | 06 | 0F | 02 | 91 | 80 | 07
[8] | 88 | 60 | 16 | DB | 62 | 00 | 43 | 08
[16] | 94 | 0B | 68 | 04 | 00 | E0 | 08 | 86
[24] | 42 | 99 | 0A | 00 | 30 | 11 | 14 |

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:09.490

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0

| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:09.490

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0

| routingInfo:
rB_Identity: | -1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:

0

| payload:
| lastSegmentShort:
sib_Type: | systemInformationBlockType11
segmentIndex: | 1
sib_Data_variable: | 000100001100001001010010011010101000011000010010101000101100011001010100101010100001001111101000100010000001010010110000100010100001010101111000

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA |  | RLC | @ 00:00:09.490

| Channel No: |  | 0 Name: BCCH

| Message Details:
| SIB repetition rate: 64

| SIB position: 60

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

lastSegmentShort:

sib_Type: systemInformationBlockType11_SIB_Type [enum=11]

segmentIndex: 1

sib_Data_variable: 000100001100001001010010011010101000011000010010101000101100011001010100101010100001001111101000100010000001010010110000100010100001010101111000

Layer 3 SDU:

[0]

00 06 B0 8F 10 C2 52 6A
[8]86 12 A2 C6 54 AA 13 E8
[16]88 14 B0 8A 15 78

#### o_SIB_PER_Encoding

RRC |  | RRC | @ 00:00:09.490

| Category: |  | TSO

| Message Details: |  | Inputs: |  | SIB: |  | sIB12: (SysInfoType12) |  | fach_MeasurementOccasionInfo: Omit

| measurementControlSysInfo:
| use_of_HCS:
| hcs_not_used:
| cellSelectQualityMeasure:
| cpich_RSCP:
| intraFreqMeasurementSysInfo: (IntraFreqMeasurementSysInfo_RSCP) Omit

interFreqMeasurementSysInfo: (InterFreqMeasurementSysInfo_RSCP) Omit

interRATMeasurementSysInfo: (InterRATMeasurementSysInfo_B) Omit

trafficVolumeMeasSysInfo: Omit

dummy: (UE_InternalMeasurementSysInfo) Omit

nonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]00 00 00 00 0

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:09.490

| Channel ID: |  | RbBcch | Cell ID: |  | 0

| Message Details: |  | CMAC_SYSINFO_Config_REQ: | cellId: | 0

| routingInfo: | rB_Identity: | -1

ratType:fdd

| configMessage: (CmacSysinfoConfigReq) | sg_REP: | 6 sg_POS: | 13 bcch_ModificationTime: | Omit

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:00:09.500

Channel ID: RbBcch
Cell ID: 0

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:0

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:00:09.500

Channel ID: RbBcch
Cell ID: 0

Message Details:

RLC_TR_DATA_REQ:

cellId:0

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

completeSIB_List:

CompleteSIBshort:

sib_Type:systemInformationBlockType12
sib_Data_variable:000000000

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:00:09.500

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 26

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

completeSIB_List:

CompleteSIB_List.element:

sib_Type: systemInformationBlockType12_SIB_Type [enum=12]

sib_Data_variable: 000000000

Layer 3 SDU:

[0]00 0E 0C 08 00 00

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:00:09.500

Channel ID: RbBcch
Cell ID: 0

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:0

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:14
bcch_ModificationTime: Omit

#### MAC_DATA_REQ

RLC MAC @ 00:00:09.510

Category: Configuration
BTS unit: 1:1
Channel No: 0 Name: BCCH
CFN: 192

Message Details:

RLC PDU size (bits):56
RLC PDU (raw):

[0]00 0E 07 17 82 80 81

#### PHY_DATA_REQ

MAC PHY @ 00:00:09.510

BTS unit: 1:1
Channel No: 0 Name: BCH
CFN: 192

Message Details:

SIB repetition period:64
SIB position:4
SIB size:246
SIB (raw):

[0]00 0E 07 17 82 80 81 07
[8]88 60 16 DB 62 00 43 08
[16]94 0B 68 04 00 E0 08 86
[24]42 99 0A 00 30 11 14 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 0E 07 17 82 80 81 07
[8]88 60 16 DB 62 00 43 08
[16]94 0B 68 04 00 E0 08 86
[24]42 99 0A 00 30 11 14

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:00:09.520

Channel ID: RbBcch
Cell ID: 0

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:0

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:00:09.520

Channel ID: RbBcch
Cell ID: 0

Message Details:

RLC_TR_DATA_REQ:

cellId:0

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

noSegment:

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:00:09.520

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 28

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

noSegment: NULL

Layer 3 SDU:

[0]00 00

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:00:09.520

Channel ID: RbBcch
Cell ID: 0

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:0

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:15
bcch_ModificationTime: Omit

#### MAC_DATA_REQ

RLC MAC @ 00:00:09.520

Category: Configuration
BTS unit: 1:1
Channel No: 0 Name: BCCH
CFN: 193

Message Details:

RLC PDU size (bits):184
RLC PDU (raw):

[0]00 0E 27 17 82 80 81 1B
[8]7A 00 00 00 05 B8 C0 00
[16]80 12 10 23 FF FF F8

#### MAC_DATA_REQ

RLC MAC @ 00:00:09.520

Category: Configuration
BTS unit: 1:1
Channel No: 0 Name: BCCH
CFN: 193

Message Details:

RLC PDU size (bits):80
RLC PDU (raw):

[0]00 0E 27 17 82 80 81 D0
[8]2C 00

#### MAC_DATA_REQ

RLC MAC @ 00:00:09.520

Category: Configuration
BTS unit: 1:1
Channel No: 0 Name: BCCH
CFN: 193

Message Details:

RLC PDU size (bits):168
RLC PDU (raw):

[0]00 0E 27 17 82 80 81 22
[8]F0 00 00 00 0B 71 80 01
[16]00 24 00 47 70

#### MAC_DATA_REQ

RLC MAC @ 00:00:09.520

Category: Configuration
BTS unit: 1:1
Channel No: 0 Name: BCCH
CFN: 193

Message Details:

RLC PDU size (bits):16
RLC PDU (raw):

[0]00 00

#### MAC_DATA_REQ

RLC MAC @ 00:00:09.520

Category: Configuration
BTS unit: 1:1
Channel No: 0 Name: BCCH
CFN: 193

Message Details:

RLC PDU size (bits):248
RLC PDU (raw):

[0]00 02 B1 20 D9 12 00 8C
[8]84 21 25 A8 82 64 53 05
[16]90 A7 0B 85 08 88 C9 54
[24]04 A1 4A 86 12 88 28

#### MAC_DATA_REQ

RLC MAC @ 00:00:09.520

Category: Configuration
BTS unit: 1:1
Channel No: 0 Name: BCCH
CFN: 193

Message Details:

RLC PDU size (bits):176
RLC PDU (raw):

[0]00 06 B0 8F 10 C2 52 6A
[8]86 12 A2 C6 54 AA 13 E8
[16]88 14 B0 8A 15 78

#### MAC_DATA_REQ

RLC MAC @ 00:00:09.520

Category: Configuration
BTS unit: 1:1
Channel No: 0 Name: BCCH
CFN: 193

Message Details:

RLC PDU size (bits):48
RLC PDU (raw):

[0]00 0E 0C 08 00 00

#### MAC_DATA_REQ

RLC MAC @ 00:00:09.530

Category: Configuration
BTS unit: 1:1
Channel No: 0 Name: BCCH
CFN: 194

Message Details:

RLC PDU size (bits):16
RLC PDU (raw):

[0]00 00

#### PHY_DATA_REQ

MAC PHY @ 00:00:09.530

BTS unit: 1:1
Channel No: 0 Name: BCH
CFN: 194

Message Details:

SIB repetition period:64
SIB position:20
SIB size:246
SIB (raw):

[0]00 0E 27 17 82 80 81 1B
[8]7A 00 00 00 05 B8 C0 00
[16]80 12 10 23 FF FF F8 86
[24]42 99 0A 00 30 11 14 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 0E 27 17 82 80 81 1B
[8]7A 00 00 00 05 B8 C0 00
[16]80 12 10 23 FF FF F8 86
[24]42 99 0A 00 30 11 14

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:00:09.540

Channel ID: RbBcch
Cell ID: 0

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:0

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:00:09.540

Channel ID: RbBcch
Cell ID: 0

Message Details:

RLC_TR_DATA_REQ:

cellId:0

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

noSegment:

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:00:09.540

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 30

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

noSegment: NULL

Layer 3 SDU:

[0]00 00

#### o_SIB_PER_Encoding

RRC RRC @ 00:00:09.540

Category: TSO

Message Details:

Inputs:

SIB:

sIB18: (SysInfoType18)

idleModePLMNIdentities: (PLMNIdentitiesOfNeighbourCells)

plmnsOfIntraFreqCellsList: Omit

plmnsOfInterFreqCellsList: Omit

plmnsOfInterRATCellsList: Omit

connectedModePLMNIdentities: (PLMNIdentitiesOfNeighbourCells) Omit

nonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]10 00 00

#### o_SIB_PER_Encoding

RRC RRC @ 00:00:09.540

Category: TSO

Message Details:

Inputs:

SIB:

sIB7: (SysInfoType7)

modeSpecificInfo:

fdd:

ul_Interference:-100

prach_Information_SIB5_List: (DynamicPersistenceLevelList)

DynamicPersistenceLevel:2

prach_Information_SIB6_List: (DynamicPersistenceLevelList)

DynamicPersistenceLevel:2

expirationTimeFactor: Omit

nonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]10 00 00 10 10 00 00 00
[8]10 00 00 01

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:00:09.540

Channel ID: RbBcch
Cell ID: 0

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:0

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:18
bcch_ModificationTime: Omit

#### MAC_DATA_REQ

RLC MAC @ 00:00:09.540

Category: Configuration
BTS unit: 1:1
Channel No: 0 Name: BCCH
CFN: 195

Message Details:

RLC PDU size (bits):16
RLC PDU (raw):

[0]00 00

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:00:09.550

Channel ID: RbBcch
Cell ID: 0

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:0

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:00:09.550

Channel ID: RbBcch
Cell ID: 0

Message Details:

RLC_TR_DATA_REQ:

cellId:0

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

completeSIB_List:

CompleteSIBshort:

sib_Type:systemInformationBlockType7
sib_Data_variable:100000101000000010000001

CompleteSIBshort:

sib_Type:systemInformationBlockType18
sib_Data_variable:100000

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:00:09.550

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 36

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

completeSIB_List:

CompleteSIB_List.element:

sib_Type: systemInformationBlockType7_SIB_Type [enum=7]

sib_Data_variable: 100000101000000010000001

CompleteSIB_List.element:

sib_Type: systemInformationBlockType18_SIB_Type [enum=26]

sib_Data_variable: 100000

Layer 3 SDU:

[0]00 0E 27 17 82 80 81 D0
[8]2C 00

#### o_SIB_PER_Encoding

RRC RRC @ 00:00:09.550

Category: TSO

Message Details:

Inputs:

SIB:

sB1: (SysInfoTypeSB1)

sib_ReferenceList:

SchedulingInformationSIB:

sib_Type: (SIB_TypeAndTag)

sysInfoType6 (CellValueTag):2

scheduling: (SchedulingInformation)

scheduling:

segCount: Omit

sib_Pos:

rep64:3

sib_PosOffsetInfo: (SibOFF_List) Omit

SchedulingInformationSIB:

sib_Type: (SIB_TypeAndTag)

sysInfoType7:

scheduling: (SchedulingInformation)

scheduling:

segCount: Omit

sib_Pos:

rep16:2

sib_PosOffsetInfo: (SibOFF_List) Omit

SchedulingInformationSIB:

sib_Type: (SIB_TypeAndTag)

sysInfoType11 (CellValueTag):2

scheduling: (SchedulingInformation)

scheduling:

segCount:2

sib_Pos:

rep64:29

sib_PosOffsetInfo: (SibOFF_List)

SibOFF:so2

SchedulingInformationSIB:

sib_Type: (SIB_TypeAndTag)

sysInfoType12 (CellValueTag):2

scheduling: (SchedulingInformation)

scheduling:

segCount: Omit

sib_Pos:

rep64:13

sib_PosOffsetInfo: (SibOFF_List) Omit

SchedulingInformationSIB:

sib_Type: (SIB_TypeAndTag)

sysInfoType18 (CellValueTag):2

scheduling: (SchedulingInformation)

scheduling:

segCount: Omit

sib_Pos:

rep64:18

sib_PosOffsetInfo: (SibOFF_List) Omit

nonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]00 01 00 00 10 10 10 00
[8]10 00 00 11 00 11 00 00
[16]01 00 10 01 01 00 11 10
[24]00 10 10 01 11 01 00 00
[32]00 00 01 01 10 10 00 10
[40]00 11 01 11 00 10 10 00
[48]10 01 00 10

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:00:09.550

Channel ID: RbBcch
Cell ID: 0

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:0

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:4
sg_POS:1
bcch_ModificationTime: Omit

#### PHY_DATA_REQ

MAC PHY @ 00:00:09.550

BTS unit: 1:1
Channel No: 0 Name: BCH
CFN: 196

Message Details:

SIB repetition period:64
SIB position:36
SIB size:246
SIB (raw):

[0]00 0E 27 17 82 80 81 D0
[8]2C 00 00 00 05 B8 C0 00
[16]80 12 10 23 FF FF F8 86
[24]42 99 0A 00 30 11 14 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 0E 27 17 82 80 81 D0
[8]2C 00 00 00 05 B8 C0 00
[16]80 12 10 23 FF FF F8 86
[24]42 99 0A 00 30 11 14

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:00:09.570

Channel ID: RbBcch
Cell ID: 0

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:0

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:00:09.570

Channel ID: RbBcch
Cell ID: 0

Message Details:

RLC_TR_DATA_REQ:

cellId:0

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

completeSIB_List:

CompleteSIBshort:

sib_Type:schedulingBlock1
sib_Data_variable:00010000101010001000001100110000010010010100111000101001110100000000010110100010001101110010100010010010

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:00:09.570

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 16

SIB position: 2

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

completeSIB_List:

CompleteSIB_List.element:

sib_Type: schedulingBlock1_SIB_Type [enum=27]

sib_Data_variable: 00010000101010001000001100110000010010010100111000101001110100000000010110100010001101110010100010010010

Layer 3 SDU:

[0]00 0E 1B 67 10 A8 83 30
[8]49 4E 29 D0 05 A2 37 28
[16]92

#### o_SIB_PER_Encoding

RRC RRC @ 00:00:09.570

Category: TSO

Message Details:

Inputs:

SIB:

mIB: (MasterInformationBlock)

mib_ValueTag:1

plmn_Type:

gsm_MAP:

plmn_Identity:

mcc:

Digit:0
Digit:0
Digit:1

mnc:

Digit:0
Digit:1

sibSb_ReferenceList:

SchedulingInformationSIBSb:

sibSb_Type: (SIBSb_TypeAndTag)

sysInfoTypeSB1 (CellValueTag):2

scheduling: (SchedulingInformation)

scheduling:

segCount: Omit

sib_Pos:

rep16:1

sib_PosOffsetInfo: (SibOFF_List) Omit

SchedulingInformationSIBSb:

sibSb_Type: (SIBSb_TypeAndTag)

sysInfoType1 (PLMN_ValueTag):2

scheduling: (SchedulingInformation)

scheduling:

segCount: Omit

sib_Pos:

rep64:11

sib_PosOffsetInfo: (SibOFF_List) Omit

SchedulingInformationSIBSb:

sibSb_Type: (SIBSb_TypeAndTag)

sysInfoType2 (CellValueTag):2

scheduling: (SchedulingInformation)

scheduling:

segCount: Omit

sib_Pos:

rep64:11

sib_PosOffsetInfo: (SibOFF_List) Omit

SchedulingInformationSIBSb:

sibSb_Type: (SIBSb_TypeAndTag)

sysInfoType3 (CellValueTag):2

scheduling: (SchedulingInformation)

scheduling:

segCount: Omit

sib_Pos:

rep64:10

sib_PosOffsetInfo: (SibOFF_List) Omit

SchedulingInformationSIBSb:

sibSb_Type: (SIBSb_TypeAndTag)

sysInfoType4 (CellValueTag):2

scheduling: (SchedulingInformation)

scheduling:

segCount: Omit

sib_Pos:

rep64:26

sib_PosOffsetInfo: (SibOFF_List) Omit

SchedulingInformationSIBSb:

sibSb_Type: (SIBSb_TypeAndTag)

sysInfoType5 (CellValueTag):2

scheduling: (SchedulingInformation)

scheduling:

segCount:3

sib_Pos:

rep64:19

sib_PosOffsetInfo: (SibOFF_List)

SibOFF:so4
SibOFF:so2

nonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]00 00 00 00 00 00 00 00
[8]01 00 00 00 00 10 01 01
[16]10 10 10 10 00 01 00 01
[24]00 00 00 00 00 00 10 00
[32]10 00 10 11 00 00 10 10
[40]00 10 00 10 11 00 01 00
[48]10 00 10 00 10 10 00 01
[56]10 10 00 10 01 10 10 00
[64]10 00 11 10 01 00 10 01
[72]00 11 00 01 00 01 00 00

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:00:09.570

Channel ID: RbBcch
Cell ID: 0

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:0

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:3
sg_POS:0
bcch_ModificationTime: Omit

#### PHY_DATA_REQ

MAC PHY @ 00:00:09.570

BTS unit: 1:1
Channel No: 0 Name: BCH
CFN: 198

Message Details:

SIB repetition period:64
SIB position:52
SIB size:246
SIB (raw):

[0]00 0E 27 17 82 80 81 22
[8]F0 00 00 00 0B 71 80 01
[16]00 24 00 47 70 FF F8 86
[24]42 99 0A 00 30 11 14 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 0E 27 17 82 80 81 22
[8]F0 00 00 00 0B 71 80 01
[16]00 24 00 47 70 FF F8 86
[24]42 99 0A 00 30 11 14

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:00:09.580

Channel ID: RbBcch
Cell ID: 0

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:0

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:00:09.580

Channel ID: RbBcch
Cell ID: 0

Message Details:

RLC_TR_DATA_REQ:

cellId:0

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

completeSIB_List:

CompleteSIBshort:

sib_Type:masterInformationBlock
sib_Data_variable:0000000000000000010000000010010110101010000100010000000000001000100010110000101000100010110001001000100010100001101000100110100010001110010010010011000100010000

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:00:09.580

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 8

SIB position: 0

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

completeSIB_List:

CompleteSIB_List.element:

sib_Type: masterInformationBlock_SIB_Type [enum=0]

sib_Data_variable: 0000000000000000010000000010010110101010000100010000000000001000100010110000101000100010110001001000100010100001101000100110100010001110010010010011000100010000

Layer 3 SDU:

[0]00 0E 00 9F 00 00 40 25
[8]AA 11 00 08 8B 0A 22 C4
[16]88 A1 A2 68 8E 49 31 10

#### MMI_CmdReq

RRC LLA @ 00:00:09.580

Message Details:

MMI_CmdReq:

cmd (IA5String):Please switch on the UE

#### PHY_DATA_REQ

MAC PHY @ 00:00:09.590

BTS unit: 1:1
Channel No: 0 Name: BCH
CFN: 200

Message Details:

SIB repetition period:64
SIB position:62
SIB size:246
SIB (raw):

[0]00 00 27 17 82 80 81 22
[8]F0 00 00 00 0B 71 80 01
[16]00 24 00 47 70 FF F8 86
[24]42 99 0A 00 30 11 14 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 00 27 17 82 80 81 22
[8]F0 00 00 00 0B 71 80 01
[16]00 24 00 47 70 FF F8 86
[24]42 99 0A 00 30 11 14

#### PHY_DATA_REQ

MAC PHY @ 00:00:09.610

BTS unit: 1:1
Channel No: 0 Name: BCH
CFN: 202

Message Details:

SIB repetition period:64
SIB position:58
SIB size:246
SIB (raw):

[0]00 02 B1 20 D9 12 00 8C
[8]84 21 25 A8 82 64 53 05
[16]90 A7 0B 85 08 88 C9 54
[24]04 A1 4A 86 12 88 28 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 02 B1 20 D9 12 00 8C
[8]84 21 25 A8 82 64 53 05
[16]90 A7 0B 85 08 88 C9 54
[24]04 A1 4A 86 12 88 28

#### PHY_DATA_REQ

MAC PHY @ 00:00:09.630

BTS unit: 1:1
Channel No: 0 Name: BCH
CFN: 204

Message Details:

SIB repetition period:64
SIB position:60
SIB size:246
SIB (raw):

[0]00 06 B0 8F 10 C2 52 6A
[8]86 12 A2 C6 54 AA 13 E8
[16]88 14 B0 8A 15 78 C9 54
[24]04 A1 4A 86 12 88 28 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 06 B0 8F 10 C2 52 6A
[8]86 12 A2 C6 54 AA 13 E8
[16]88 14 B0 8A 15 78 C9 54
[24]04 A1 4A 86 12 88 28

#### PHY_DATA_REQ

MAC PHY @ 00:00:09.650

BTS unit: 1:1
Channel No: 0 Name: BCH
CFN: 206

Message Details:

SIB repetition period:64
SIB position:26
SIB size:246
SIB (raw):

[0]00 0E 0C 08 00 00 52 6A
[8]86 12 A2 C6 54 AA 13 E8
[16]88 14 B0 8A 15 78 C9 54
[24]04 A1 4A 86 12 88 28 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 0E 0C 08 00 00 52 6A
[8]86 12 A2 C6 54 AA 13 E8
[16]88 14 B0 8A 15 78 C9 54
[24]04 A1 4A 86 12 88 28

#### MAC_DATA_REQ

RLC MAC @ 00:00:09.670

Category: Configuration
BTS unit: 1:1
Channel No: 0 Name: BCCH
CFN: 208

Message Details:

RLC PDU size (bits):80
RLC PDU (raw):

[0]00 0E 27 17 82 80 81 D0
[8]2C 00

#### MAC_DATA_REQ

RLC MAC @ 00:00:09.670

Category: Configuration
BTS unit: 1:1
Channel No: 0 Name: BCCH
CFN: 208

Message Details:

RLC PDU size (bits):136
RLC PDU (raw):

[0]00 0E 1B 67 10 A8 83 30
[8]49 4E 29 D0 05 A2 37 28
[16]92

#### MAC_DATA_REQ

RLC MAC @ 00:00:09.670

Category: Configuration
BTS unit: 1:1
Channel No: 0 Name: BCCH
CFN: 208

Message Details:

RLC PDU size (bits):192
RLC PDU (raw):

[0]00 0E 00 9F 00 00 40 25
[8]AA 11 00 08 8B 0A 22 C4
[16]88 A1 A2 68 8E 49 31 10

#### PHY_DATA_REQ

MAC PHY @ 00:00:09.670

BTS unit: 1:1
Channel No: 0 Name: BCH
CFN: 208

Message Details:

SIB repetition period:64
SIB position:28
SIB size:246
SIB (raw):

[0]00 00 0C 08 00 00 52 6A
[8]86 12 A2 C6 54 AA 13 E8
[16]88 14 B0 8A 15 78 C9 54
[24]04 A1 4A 86 12 88 28 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 00 0C 08 00 00 52 6A
[8]86 12 A2 C6 54 AA 13 E8
[16]88 14 B0 8A 15 78 C9 54
[24]04 A1 4A 86 12 88 28

#### PHY_DATA_REQ

MAC PHY @ 00:00:09.690

BTS unit: 1:1
Channel No: 0 Name: BCH
CFN: 210

Message Details:

SIB repetition period:64
SIB position:30
SIB size:246
SIB (raw):

[0]00 00 0C 08 00 00 52 6A
[8]86 12 A2 C6 54 AA 13 E8
[16]88 14 B0 8A 15 78 C9 54
[24]04 A1 4A 86 12 88 28 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 00 0C 08 00 00 52 6A
[8]86 12 A2 C6 54 AA 13 E8
[16]88 14 B0 8A 15 78 C9 54
[24]04 A1 4A 86 12 88 28

#### PHY_DATA_REQ

MAC PHY @ 00:00:09.710

BTS unit: 1:1
Channel No: 0 Name: BCH
CFN: 212

Message Details:

SIB repetition period:64
SIB position:36
SIB size:246
SIB (raw):

[0]00 0E 27 17 82 80 81 D0
[8]2C 00 A2 C6 54 AA 13 E8
[16]88 14 B0 8A 15 78 C9 54
[24]04 A1 4A 86 12 88 28 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 0E 27 17 82 80 81 D0
[8]2C 00 A2 C6 54 AA 13 E8
[16]88 14 B0 8A 15 78 C9 54
[24]04 A1 4A 86 12 88 28

#### PHY_DATA_REQ

MAC PHY @ 00:00:09.730

BTS unit: 1:1
Channel No: 0 Name: BCH
CFN: 214

Message Details:

SIB repetition period:16
SIB position:2
SIB size:246
SIB (raw):

[0]00 0E 1B 67 10 A8 83 30
[8]49 4E 29 D0 05 A2 37 28
[16]92 14 B0 8A 15 78 C9 54
[24]04 A1 4A 86 12 88 28 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 0E 1B 67 10 A8 83 30
[8]49 4E 29 D0 05 A2 37 28
[16]92 14 B0 8A 15 78 C9 54
[24]04 A1 4A 86 12 88 28

#### PHY_DATA_REQ

MAC PHY @ 00:00:09.750

BTS unit: 1:1
Channel No: 0 Name: BCH
CFN: 216

Message Details:

SIB repetition period:8
SIB position:0
SIB size:246
SIB (raw):

[0]00 0E 00 9F 00 00 40 25
[8]AA 11 00 08 8B 0A 22 C4
[16]88 A1 A2 68 8E 49 31 10
[24]04 A1 4A 86 12 88 28 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 0E 00 9F 00 00 40 25
[8]AA 11 00 08 8B 0A 22 C4
[16]88 A1 A2 68 8E 49 31 10
[24]04 A1 4A 86 12 88 28

#### MMI_CmdCnf

LLA RRC @ 00:00:10.680

Message Details:

MMI_CmdCnf:

result:true
resultString (IA5String): Omit

#### PHY_DATA_IND

PHY MAC @ 00:00:34.120

BTS unit: 1:1
Channel No: 0 Name: U_RACH
CFN: 73

Message Details:

TFI:0
TB set size:168
TB size:168
TB set (raw):

[0]08 82 61 D9 50 C0 04 02
[8]00 02 0A C0 00 00 00 00
[16]00 00 00 00 00 00

TB set (decoded):

TB 0:

TCTF:0
MAC SDU (166 bits):

[0]22 09 87 65 43 00 10 08
[8]00 08 2B 00 00 00 00 00
[16]00 00 00 00 00

#### MAC_DATA_IND

MAC RLC @ 00:00:34.120

Category: Configuration
BTS unit: 1:1
Channel No: 0 Name: CCCH
CFN: 73

Message Details:

RLC PDU size (bits):166
RLC PDU (raw):

[0]22 09 87 65 43 00 10 08
[8]00 08 2B 00 00 00 00 00
[16]00 00 00 00 00

#### RLC_TR_DATA_IND: rrcConnectionRequest

RLC LLA @ 00:00:34.140

Channel No: 0 Name: CCCH

Message Details:

UL_CCCH_Message:

integrityCheckInfo: Omitted

message:

rrcConnectionRequest:

initialUE_Identity:

p_TMSI_and_RAI:

p_TMSI: 00001001100001110110010101000011

rai:

lai:

plmn_Identity:

mcc:

MCC.element: 0

MCC.element: 0

MCC.element: 1

mnc:

MNC.element: 0

MNC.element: 1

lac: 0000000000000001

rac: 00000101

establishmentCause: registration_EstablishmentCause [enum=12]

protocolErrorIndicator: noError_ProtocolErrorIndicator [enum=0]

measuredResultsOnRACH: Omitted

v3d0NonCriticalExtensions: Omitted

Layer 3 SDU:

[0]22 09 87 65 43 00 10 08
[8]00 08 2B 00 00 00 00 00
[16]00 00 00 00 00

#### RLC_TR_DATA_IND

LLA RRC @ 00:00:34.140

Channel ID: Rb0
Cell ID: 0

Message Details:

RLC_TR_DATA_IND:

cellId:0

routingInfo:

rB_Identity:0

tM_message:

uL_CCCH_Message:

integrityCheckInfo: Omit

message: (UL_CCCH_MessageType)

rrcConnectionRequest:

initialUE_Identity:

p_TMSI_and_RAI: (P_TMSI_and_RAI_GSM_MAP)

p_TMSI (P_TMSI_GSM_MAP):00001001100001110110010101000011

rai:

lai:

plmn_Identity:

mcc:

Digit:0
Digit:0
Digit:1

mnc:

Digit:0
Digit:1

lac:0000000000000001

rac (RoutingAreaCode):00000101

establishmentCause:registration
protocolErrorIndicator:noError

measuredResultsOnRACH: Omit

v3d0NonCriticalExtensions: Omit

#### RLC_UM_DATA_REQ

RRC LLA @ 00:00:34.140

Channel ID: Rb0
Cell ID: 0

Message Details:

RLC_UM_DATA_REQ:

cellId:0

routingInfo:

rB_Identity:0

uM_message:

dL_CCCH_Message:

integrityCheckInfo: Omit

message: (DL_CCCH_MessageType)

rrcConnectionSetup:

r3:

rrcConnectionSetup_r3: (RRCConnectionSetup_r3_IEs)

initialUE_Identity:

p_TMSI_and_RAI: (P_TMSI_and_RAI_GSM_MAP)

p_TMSI (P_TMSI_GSM_MAP):00001001100001110110010101000011

rai:

lai:

plmn_Identity:

mcc:

Digit:0
Digit:0
Digit:1

mnc:

Digit:0
Digit:1

lac:0000000000000001

rac (RoutingAreaCode):00000101

rrc_TransactionIdentifier:0
activationTime: Omit

new_U_RNTI: (U_RNTI)

srnc_Identity:000000000001
s_RNTI:00000000000000000001

new_c_RNTI (C_RNTI): Omit
rrc_StateIndicator:cell_DCH
utran_DRX_CycleLengthCoeff (UTRAN_DRX_CycleLengthCoefficient):9

capabilityUpdateRequirement:

ue_RadioCapabilityFDDUpdateRequirement:true
ue_RadioCapabilityTDDUpdateRequirement:false

systemSpecificCapUpdateReqList:

SystemSpecificCapUpdateReq:gsm

srb_InformationSetupList: (SRB_InformationSetupList2)

SRB_InformationSetup:

rb_Identity: Omit

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_UM_RLC_Mode:

transmissionRLC_Discard: Omit

dl_RLC_Mode:

dl_UM_RLC_Mode:

rb_MappingInfo:

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

dch (TransportChannelIdentity):5

logicalChannelIdentity:1

rlc_SizeList:

configured:

mac_LogicalChannelPriority:1

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

dch (TransportChannelIdentity):10

logicalChannelIdentity:1

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

rach:

logicalChannelIdentity:1

rlc_SizeList:

explicitList: (RLC_SizeExplicitList)

RLC_SizeInfo:

rlc_SizeIndex:1

mac_LogicalChannelPriority:1

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

fach:

logicalChannelIdentity:1

SRB_InformationSetup:

rb_Identity: Omit

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

rb_MappingInfo:

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

dch (TransportChannelIdentity):5

logicalChannelIdentity:2

rlc_SizeList:

configured:

mac_LogicalChannelPriority:2

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

dch (TransportChannelIdentity):10

logicalChannelIdentity:2

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

rach:

logicalChannelIdentity:2

rlc_SizeList:

explicitList: (RLC_SizeExplicitList)

RLC_SizeInfo:

rlc_SizeIndex:1

mac_LogicalChannelPriority:2

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

fach:

logicalChannelIdentity:2

SRB_InformationSetup:

rb_Identity: Omit

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

rb_MappingInfo:

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

dch (TransportChannelIdentity):5

logicalChannelIdentity:3

rlc_SizeList:

configured:

mac_LogicalChannelPriority:3

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

dch (TransportChannelIdentity):10

logicalChannelIdentity:3

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

rach:

logicalChannelIdentity:3

rlc_SizeList:

explicitList: (RLC_SizeExplicitList)

RLC_SizeInfo:

rlc_SizeIndex:1

mac_LogicalChannelPriority:3

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

fach:

logicalChannelIdentity:3

SRB_InformationSetup:

rb_Identity: Omit

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

rb_MappingInfo:

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

dch (TransportChannelIdentity):5

logicalChannelIdentity:4

rlc_SizeList:

configured:

mac_LogicalChannelPriority:4

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

dch (TransportChannelIdentity):10

logicalChannelIdentity:4

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

rach:

logicalChannelIdentity:4

rlc_SizeList:

explicitList: (RLC_SizeExplicitList)

RLC_SizeInfo:

rlc_SizeIndex:1

mac_LogicalChannelPriority:4

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

fach:

logicalChannelIdentity:4

ul_CommonTransChInfo:

tfc_Subset: Omit

prach_TFCS: (TFCS) Omit

modeSpecificInfo:

fdd:

ul_TFCS: (TFCS)

normalTFCI_Signalling: (ExplicitTFCS_Configuration)

complete: (TFCS_ReconfAdd)

ctfcSize:

ctfc2Bit:

:

ctfc2:0

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc2:1

powerOffsetInformation:

gainFactorInformation:

signalledGainFactors:

modeSpecificInfo:

fdd:

gainFactorBetaC (GainFactor):11

gainFactorBetaD (GainFactor):15
referenceTFC_ID:0

powerOffsetPp_m: Omit

ul_AddReconfTransChInfoList:

UL_AddReconfTransChInformation:

ul_TransportChannelType (UL_TrCH_Type):dch
transportChannelIdentity:5

transportFormatSet:

dedicatedTransChTFS:

tti:

tti10: (DedicatedDynamicTF_InfoList)

DedicatedDynamicTF_Info:

rlc_Size:

bitMode: (BitModeRLC_SizeInfo)

sizeType2:

part1:2
part2: Omit

numberOfTbSizeList:

NumberOfTransportBlocks:

zero:

NumberOfTransportBlocks:

one:

logicalChannelList:

allSizes:

semistaticTF_Information:

channelCodingType:

convolutional (CodingRate):third

rateMatchingAttribute:192
crc_Size:crc16

dl_CommonTransChInfo:

sccpch_TFCS: (TFCS) Omit

modeSpecificInfo:

fdd:

dl_Parameters:

sameAsUL:

dl_AddReconfTransChInfoList:

DL_AddReconfTransChInformation:

dl_TransportChannelType (DL_TrCH_Type):dch
dl_transportChannelIdentity (TransportChannelIdentity):10

tfs_SignallingMode:

sameAsULTrCH: (UL_TransportChannelIdentity)

ul_TransportChannelType (UL_TrCH_Type):dch
ul_TransportChannelIdentity (TransportChannelIdentity):5

dch_QualityTarget: (QualityTarget)

bler_QualityValue:-20

dummy: (TM_SignallingInfo) Omit

frequencyInfo: Omit

maxAllowedUL_TX_Power: Omit

ul_ChannelRequirement:

ul_DPCH_Info:

ul_DPCH_PowerControlInfo:

fdd:

dpcch_PowerOffset:-40
pc_Preamble:1
sRB_delay:7

powerControlAlgorithm:

algorithm1 (TPC_StepSizeFDD):0

modeSpecificInfo:

fdd:

scramblingCodeType:longSC
scramblingCode (UL_ScramblingCode):0
numberOfDPDCH: Omit
spreadingFactor:sf64
tfci_Existence:true
numberOfFBI_Bits: Omit
puncturingLimit:pl1

dl_CommonInformation:

dl_DPCH_InfoCommon:

cfnHandling:

initialise:

cfntargetsfnframeoffset: Omit

modeSpecificInfo:

fdd:

dl_DPCH_PowerControlInfo:

modeSpecificInfo:

fdd:

dpc_Mode:singleTPC

powerOffsetPilot_pdpdch:0

dl_rate_matching_restriction: Omit

spreadingFactorAndPilot: (SF512_AndPilot)

sfd128 (PilotBits128):pb4

positionFixedOrFlexible:fixed
tfci_Existence:false

modeSpecificInfo:

fdd:

defaultDPCH_OffsetValue (DefaultDPCH_OffsetValueFDD):0

dpch_CompressedModeInfo: Omit

tx_DiversityMode:noDiversity

ssdt_Information: Omit

dl_InformationPerRL_List:

DL_InformationPerRL:

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode:100

pdsch_SHO_DCH_Info: Omit

pdsch_CodeMapping: Omit

dl_DPCH_InfoPerRL:

fdd:

pCPICH_UsageForChannelEst:mayBeUsed
dpch_FrameOffset:0

secondaryCPICH_Info: Omit

dl_ChannelisationCodeList:

DL_ChannelisationCode:

secondaryScramblingCode:1

sf_AndCodeNumber: (SF512_AndCodeNumber)

sf128:0

scramblingCodeChange:noCodeChange

tpc_CombinationIndex:0
ssdt_CellIdentity: Omit
closedLoopTimingAdjMode: Omit

sccpch_InfoforFACH: Omit

laterNonCriticalExtensions: Omit

specialLI:true

#### RLC_UM_DATA_REQ: rrcConnectionSetup

LLA RLC @ 00:00:34.160

Channel No: 1 Name: CCCH

Message Details:

DL_CCCH_Message:

integrityCheckInfo: Omitted

message:

rrcConnectionSetup:

r3:

rrcConnectionSetup_r3:

initialUE_Identity:

p_TMSI_and_RAI:

p_TMSI: 00001001100001110110010101000011

rai:

lai:

plmn_Identity:

mcc:

MCC.element: 0

MCC.element: 0

MCC.element: 1

mnc:

MNC.element: 0

MNC.element: 1

lac: 0000000000000001

rac: 00000101

rrc_TransactionIdentifier: 0

activationTime: Omitted

new_U_RNTI:

srnc_Identity: 000000000001

s_RNTI: 00000000000000000001

new_c_RNTI: Omitted

rrc_StateIndicator: cell_DCH_RRC_StateIndicator [enum=0]

utran_DRX_CycleLengthCoeff: 9

capabilityUpdateRequirement:

ue_RadioCapabilityFDDUpdateRequirement: 1

ue_RadioCapabilityTDDUpdateRequirement: 0

systemSpecificCapUpdateReqList:

SystemSpecificCapUpdateReqList.element: gsm_SystemSpecificCapUpdateReq [enum=0]

srb_InformationSetupList:

SRB_InformationSetupList2.element:

rb_Identity: Omitted

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_UM_RLC_Mode:

transmissionRLC_Discard: Omitted

dl_RLC_Mode:

dl_UM_RLC_Mode: NULL

rb_MappingInfo:

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

dch: 5

logicalChannelIdentity: 1

rlc_SizeList:

configured: NULL

mac_LogicalChannelPriority: 1

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

dch: 10

logicalChannelIdentity: 1

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

rach: NULL

logicalChannelIdentity: 1

rlc_SizeList:

explicitList:

RLC_SizeExplicitList.element:

rlc_SizeIndex: 1

mac_LogicalChannelPriority: 1

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

fach: NULL

logicalChannelIdentity: 1

SRB_InformationSetupList2.element:

rb_Identity: Omitted

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard: dat15_MaxDAT [enum=10]

transmissionWindowSize: tw32_TransmissionWindowSize [enum=3]

timerRST: tr500_TimerRST [enum=9]

max_RST: rst1_MaxRST [enum=0]

pollingInfo:

timerPollProhibit: tpp200_TimerPollProhibit [enum=19]

timerPoll: tp200_TimerPoll [enum=19]

poll_PDU: Omitted

poll_SDU: sdu1_Poll_SDU [enum=0]

lastTransmissionPDU_Poll: 1

lastRetransmissionPDU_Poll: 1

pollWindow: pw99_PollWindow [enum=7]

timerPollPeriodic: Omitted

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery: 1

receivingWindowSize: rw32_ReceivingWindowSize [enum=3]

dl_RLC_StatusInfo:

timerStatusProhibit: tsp200_TimerStatusProhibit [enum=19]

timerEPC: Omitted

missingPDU_Indicator: 1

timerStatusPeriodic: Omitted

rb_MappingInfo:

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

dch: 5

logicalChannelIdentity: 2

rlc_SizeList:

configured: NULL

mac_LogicalChannelPriority: 2

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

dch: 10

logicalChannelIdentity: 2

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

rach: NULL

logicalChannelIdentity: 2

rlc_SizeList:

explicitList:

RLC_SizeExplicitList.element:

rlc_SizeIndex: 1

mac_LogicalChannelPriority: 2

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

fach: NULL

logicalChannelIdentity: 2

SRB_InformationSetupList2.element:

rb_Identity: Omitted

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard: dat15_MaxDAT [enum=10]

transmissionWindowSize: tw32_TransmissionWindowSize [enum=3]

timerRST: tr500_TimerRST [enum=9]

max_RST: rst1_MaxRST [enum=0]

pollingInfo:

timerPollProhibit: tpp200_TimerPollProhibit [enum=19]

timerPoll: tp200_TimerPoll [enum=19]

poll_PDU: Omitted

poll_SDU: sdu1_Poll_SDU [enum=0]

lastTransmissionPDU_Poll: 1

lastRetransmissionPDU_Poll: 1

pollWindow: pw99_PollWindow [enum=7]

timerPollPeriodic: Omitted

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery: 1

receivingWindowSize: rw32_ReceivingWindowSize [enum=3]

dl_RLC_StatusInfo:

timerStatusProhibit: tsp200_TimerStatusProhibit [enum=19]

timerEPC: Omitted

missingPDU_Indicator: 1

timerStatusPeriodic: Omitted

rb_MappingInfo:

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

dch: 5

logicalChannelIdentity: 3

rlc_SizeList:

configured: NULL

mac_LogicalChannelPriority: 3

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

dch: 10

logicalChannelIdentity: 3

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

rach: NULL

logicalChannelIdentity: 3

rlc_SizeList:

explicitList:

RLC_SizeExplicitList.element:

rlc_SizeIndex: 1

mac_LogicalChannelPriority: 3

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

fach: NULL

logicalChannelIdentity: 3

SRB_InformationSetupList2.element:

rb_Identity: Omitted

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard: dat15_MaxDAT [enum=10]

transmissionWindowSize: tw32_TransmissionWindowSize [enum=3]

timerRST: tr500_TimerRST [enum=9]

max_RST: rst1_MaxRST [enum=0]

pollingInfo:

timerPollProhibit: tpp200_TimerPollProhibit [enum=19]

timerPoll: tp200_TimerPoll [enum=19]

poll_PDU: Omitted

poll_SDU: sdu1_Poll_SDU [enum=0]

lastTransmissionPDU_Poll: 1

lastRetransmissionPDU_Poll: 1

pollWindow: pw99_PollWindow [enum=7]

timerPollPeriodic: Omitted

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery: 1

receivingWindowSize: rw32_ReceivingWindowSize [enum=3]

dl_RLC_StatusInfo:

timerStatusProhibit: tsp200_TimerStatusProhibit [enum=19]

timerEPC: Omitted

missingPDU_Indicator: 1

timerStatusPeriodic: Omitted

rb_MappingInfo:

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

dch: 5

logicalChannelIdentity: 4

rlc_SizeList:

configured: NULL

mac_LogicalChannelPriority: 4

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

dch: 10

logicalChannelIdentity: 4

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

rach: NULL

logicalChannelIdentity: 4

rlc_SizeList:

explicitList:

RLC_SizeExplicitList.element:

rlc_SizeIndex: 1

mac_LogicalChannelPriority: 4

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

fach: NULL

logicalChannelIdentity: 4

ul_CommonTransChInfo:

tfc_Subset: Omitted

prach_TFCS: Omitted

modeSpecificInfo:

fdd:

ul_TFCS:

normalTFCI_Signalling:

complete:

ctfcSize:

ctfc2Bit:

ctfc2Bit.noName:

ctfc2: 0

powerOffsetInformation:

gainFactorInformation:

computedGainFactors: 0

powerOffsetPp_m: Omitted

ctfc2Bit.noName:

ctfc2: 1

powerOffsetInformation:

gainFactorInformation:

signalledGainFactors:

modeSpecificInfo:

fdd:

gainFactorBetaC: 11

gainFactorBetaD: 15

referenceTFC_ID: 0

powerOffsetPp_m: Omitted

ul_AddReconfTransChInfoList:

UL_AddReconfTransChInfoList.element:

ul_TransportChannelType: dch_UL_TrCH_Type [enum=0]

transportChannelIdentity: 5

transportFormatSet:

dedicatedTransChTFS:

tti:

tti10:

DedicatedDynamicTF_InfoList.element:

rlc_Size:

bitMode:

sizeType2:

part1: 2

part2: Omitted

numberOfTbSizeList:

numberOfTbSizeList.element:

zero: NULL

numberOfTbSizeList.element:

one: NULL

logicalChannelList:

allSizes: NULL

semistaticTF_Information:

channelCodingType:

convolutional: third_CodingRate [enum=1]

rateMatchingAttribute: 192

crc_Size: crc16_CRC_Size [enum=3]

dl_CommonTransChInfo:

sccpch_TFCS: Omitted

modeSpecificInfo:

fdd:

dl_Parameters:

sameAsUL: NULL

dl_AddReconfTransChInfoList:

DL_AddReconfTransChInfoList.element:

dl_TransportChannelType: dch_DL_TrCH_Type [enum=0]

dl_transportChannelIdentity: 10

tfs_SignallingMode:

sameAsULTrCH:

ul_TransportChannelType: dch_UL_TrCH_Type [enum=0]

ul_TransportChannelIdentity: 5

dch_QualityTarget:

bler_QualityValue: -20

dummy: Omitted

frequencyInfo: Omitted

maxAllowedUL_TX_Power: Omitted

ul_ChannelRequirement:

ul_DPCH_Info:

ul_DPCH_PowerControlInfo:

fdd:

dpcch_PowerOffset: -40

pc_Preamble: 1

sRB_delay: 7

powerControlAlgorithm:

algorithm1: 0

modeSpecificInfo:

fdd:

scramblingCodeType: longSC_ScramblingCodeType [enum=1]

scramblingCode: 0

numberOfDPDCH: Default

spreadingFactor: sf64_SpreadingFactor [enum=4]

tfci_Existence: 1

numberOfFBI_Bits: Omitted

puncturingLimit: pl1_PuncturingLimit [enum=15]

dl_CommonInformation:

dl_DPCH_InfoCommon:

cfnHandling:

initialise:

cfntargetsfnframeoffset: Omitted

modeSpecificInfo:

fdd:

dl_DPCH_PowerControlInfo:

modeSpecificInfo:

fdd:

dpc_Mode: singleTPC_DPC_Mode [enum=0]

powerOffsetPilot_pdpdch: 0

dl_rate_matching_restriction: Omitted

spreadingFactorAndPilot:

sfd128: pb4_PilotBits128 [enum=0]

positionFixedOrFlexible: fixed_PositionFixedOrFlexible [enum=0]

tfci_Existence: 0

modeSpecificInfo:

fdd:

defaultDPCH_OffsetValue: 0

dpch_CompressedModeInfo: Omitted

tx_DiversityMode: noDiversity_TX_DiversityMode [enum=0]

ssdt_Information: Omitted

dl_InformationPerRL_List:

DL_InformationPerRL_List.element:

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode: 100

pdsch_SHO_DCH_Info: Omitted

pdsch_CodeMapping: Omitted

dl_DPCH_InfoPerRL:

fdd:

pCPICH_UsageForChannelEst: mayBeUsed_PCPICH_UsageForChannelEst [enum=0]

dpch_FrameOffset: 0

secondaryCPICH_Info: Omitted

dl_ChannelisationCodeList:

DL_ChannelisationCodeList.element:

secondaryScramblingCode: 1

sf_AndCodeNumber:

sf128: 0

scramblingCodeChange: noCodeChange_ScramblingCodeChange [enum=1]

tpc_CombinationIndex: 0

ssdt_CellIdentity: Omitted

closedLoopTimingAdjMode: Omitted

sccpch_InfoforFACH: Omitted

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]30 E7 41 30 EC A8 60 02
[8]01 00 01 05 00 04 00 00
[16]4D 82 69 3A 10 10 89 0D
[24]42 00 02 81 9E 8E 46 C9
[32]A6 7C 9C 4E 74 20 A5 12
[40]3A 8C 00 15 13 3D 1C 8D
[48]93 4C F9 38 9C E8 42 52
[56]24 B5 28 00 4A 46 7A 39
[64]1B 26 99 F2 71 39 D0 86
[72]B4 49 EA 70 00 D4 C8 00
[80]06 25 2B F0 02 00 08 82
[88]23 BF 66 08 98 95 A5 47
[96]82 00 00 01 3F 90 0A 14
[104]00 02 06 40 00 0C 28 08

#### CMAC Configuration REQ

LLA MAC @ 00:00:34.170

BTS unit: 1:1
Channel No: 0 Name: S_CCPCH
CFN: 98

Message Details:

Configuration Parameters:

Number Of Transport Channels:3

Transport Channels:

Item Number 0:

Transport Channel Parameters:

Transport Channel:

Name:PCH
Identity:0

TTI (ms):10
EP Type:1/2 Rate Convolutional Coding
CRC Size:16
RM Attribute:230
First Interleave:On
Number Of Transport Formats:2

Transport Format Set:

Transport Format 0:

Number Of Transport Blocks:0
Transport Block Size In Bits:240

Transport Format 1:

Number Of Transport Blocks:1
Transport Block Size In Bits:240

Number Of Logical Channels:1

Logical Channels:

Item Number 0:

Logical Channel:

Name:PCCH
Identity:0

Priority:1
CT Length:0
CT Value:0
TCTF Length:0
TCTF Value:0
UE ID Type:Not used
UE ID:0

Item Number 1:

Transport Channel Parameters:

Transport Channel:

Name:FACH
Identity:0

TTI (ms):10
EP Type:1/2 Rate Convolutional Coding
CRC Size:16
RM Attribute:220
First Interleave:On
Number Of Transport Formats:3

Transport Format Set:

Transport Format 0:

Number Of Transport Blocks:0
Transport Block Size In Bits:168

Transport Format 1:

Number Of Transport Blocks:1
Transport Block Size In Bits:168

Transport Format 2:

Number Of Transport Blocks:2
Transport Block Size In Bits:168

Number Of Logical Channels:1

Logical Channels:

Item Number 0:

Logical Channel:

Name:CCCH
Identity:1

Priority:1
CT Length:0
CT Value:0
TCTF Length:8
TCTF Value:64
UE ID Type:Not used
UE ID:0

Item Number 2:

Transport Channel Parameters:

Transport Channel:

Name:FACH
Identity:1

TTI (ms):10
EP Type:Turbo Coding
CRC Size:16
RM Attribute:130
First Interleave:On
Number Of Transport Formats:2

Transport Format Set:

Transport Format 0:

Number Of Transport Blocks:0
Transport Block Size In Bits:360

Transport Format 1:

Number Of Transport Blocks:1
Transport Block Size In Bits:360

Number Of Logical Channels:0

Active Flag:1

Transport Format Combination Set:

Number Of Transport Format Combinations:8

Transport Format Combinations 0:

Transport Format:0
Transport Format:0
Transport Format:0

Transport Format Combinations 1:

Transport Format:1
Transport Format:0
Transport Format:0

Transport Format Combinations 2:

Transport Format:0
Transport Format:1
Transport Format:0

Transport Format Combinations 3:

Transport Format:1
Transport Format:1
Transport Format:0

Transport Format Combinations 4:

Transport Format:0
Transport Format:2
Transport Format:0

Transport Format Combinations 5:

Transport Format:1
Transport Format:2
Transport Format:0

Transport Format Combinations 6:

Transport Format:0
Transport Format:0
Transport Format:1

Transport Format Combinations 7:

Transport Format:0
Transport Format:1
Transport Format:1

#### CMAC Configuration CNF

MAC LLA @ 00:00:34.170

BTS unit: 1:1
Channel No: 0 Name: S_CCPCH
CFN: 98

Message Details:

#### MAC_DATA_REQ

RLC MAC @ 00:00:34.190

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: CCCH
CFN: 100

Message Details:

RLC PDU size (bits):160
RLC PDU (raw):

[0]01 F8 30 E7 41 30 EC A8
[8]60 02 01 00 01 05 00 04
[16]00 00 4D 82

RLC PDU (decoded):

Sequence number:0
Length indicator 0 (octets):124 (the first data octet in this RLC PDU is the first octet of a RLC SDU)
Segment associated with length indicator 0 (0 octets):

Last segment, not associated with any length indicators (18 octets):

[0]30 E7 41 30 EC A8 60 02
[8]01 00 01 05 00 04 00 00
[16]4D 82

#### MAC_DATA_REQ

RLC MAC @ 00:00:34.190

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: CCCH
CFN: 100

Message Details:

RLC PDU size (bits):160
RLC PDU (raw):

[0]02 69 3A 10 10 89 0D 42
[8]00 02 81 9E 8E 46 C9 A6
[16]7C 9C 4E 74

RLC PDU (decoded):

Sequence number:1
Last segment, not associated with any length indicators (19 octets):

[0]69 3A 10 10 89 0D 42 00
[8]02 81 9E 8E 46 C9 A6 7C
[16]9C 4E 74

#### MAC_DATA_REQ

RLC MAC @ 00:00:34.190

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: CCCH
CFN: 100

Message Details:

RLC PDU size (bits):160
RLC PDU (raw):

[0]04 20 A5 12 3A 8C 00 15
[8]13 3D 1C 8D 93 4C F9 38
[16]9C E8 42 52

RLC PDU (decoded):

Sequence number:2
Last segment, not associated with any length indicators (19 octets):

[0]20 A5 12 3A 8C 00 15 13
[8]3D 1C 8D 93 4C F9 38 9C
[16]E8 42 52

#### MAC_DATA_REQ

RLC MAC @ 00:00:34.190

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: CCCH
CFN: 100

Message Details:

RLC PDU size (bits):160
RLC PDU (raw):

[0]06 24 B5 28 00 4A 46 7A
[8]39 1B 26 99 F2 71 39 D0
[16]86 B4 49 EA

RLC PDU (decoded):

Sequence number:3
Last segment, not associated with any length indicators (19 octets):

[0]24 B5 28 00 4A 46 7A 39
[8]1B 26 99 F2 71 39 D0 86
[16]B4 49 EA

#### MAC_DATA_REQ

RLC MAC @ 00:00:34.190

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: CCCH
CFN: 100

Message Details:

RLC PDU size (bits):160
RLC PDU (raw):

[0]08 70 00 D4 C8 00 06 25
[8]2B F0 02 00 08 82 23 BF
[16]66 08 98 95

RLC PDU (decoded):

Sequence number:4
Last segment, not associated with any length indicators (19 octets):

[0]70 00 D4 C8 00 06 25 2B
[8]F0 02 00 08 82 23 BF 66
[16]08 98 95

#### MAC_DATA_REQ

RLC MAC @ 00:00:34.190

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: CCCH
CFN: 100

Message Details:

RLC PDU size (bits):160
RLC PDU (raw):

[0]0B 24 A5 47 82 00 00 01
[8]3F 90 0A 14 00 02 06 40
[16]00 0C 28 08

RLC PDU (decoded):

Sequence number:5
Length indicator 0 (octets):18
Segment associated with length indicator 0 (18 octets):

[0]A5 47 82 00 00 01 3F 90
[8]0A 14 00 02 06 40 00 0C
[16]28 08

#### PHY_DATA_REQ

MAC PHY @ 00:00:34.190

BTS unit: 1:1
Channel No: 0 Name: FACH
CFN: 100

Message Details:

TFI:2
TB set size:336
TB size:168
TB set (raw, each TB word aligned):

[0]40 01 F8 30 E7 41 30 EC
[8]A8 60 02 01 00 01 05 00
[16]04 00 00 4D 82 00 40 02
[24]69 3A 10 10 89 0D 42 00
[32]02 81 9E 8E 46 C9 A6 7C
[40]9C 4E 74 00

TB set (decoded):

TB 0:

TCTF:64
MAC SDU (160 bits):

[0]01 F8 30 E7 41 30 EC A8
[8]60 02 01 00 01 05 00 04
[16]00 00 4D 82

TB 1:

TCTF:64
MAC SDU (160 bits):

[0]02 69 3A 10 10 89 0D 42
[8]00 02 81 9E 8E 46 C9 A6
[16]7C 9C 4E 74

#### PHY_DATA_REQ

MAC PHY @ 00:00:34.200

BTS unit: 1:1
Channel No: 0 Name: FACH
CFN: 101

Message Details:

TFI:2
TB set size:336
TB size:168
TB set (raw, each TB word aligned):

[0]40 04 20 A5 12 3A 8C 00
[8]15 13 3D 1C 8D 93 4C F9
[16]38 9C E8 42 52 00 40 06
[24]24 B5 28 00 4A 46 7A 39
[32]1B 26 99 F2 71 39 D0 86
[40]B4 49 EA 00

TB set (decoded):

TB 0:

TCTF:64
MAC SDU (160 bits):

[0]04 20 A5 12 3A 8C 00 15
[8]13 3D 1C 8D 93 4C F9 38
[16]9C E8 42 52

TB 1:

TCTF:64
MAC SDU (160 bits):

[0]06 24 B5 28 00 4A 46 7A
[8]39 1B 26 99 F2 71 39 D0
[16]86 B4 49 EA

#### PHY_DATA_REQ

MAC PHY @ 00:00:34.210

BTS unit: 1:1
Channel No: 0 Name: FACH
CFN: 102

Message Details:

TFI:2
TB set size:336
TB size:168
TB set (raw, each TB word aligned):

[0]40 08 70 00 D4 C8 00 06
[8]25 2B F0 02 00 08 82 23
[16]BF 66 08 98 95 00 40 0B
[24]24 A5 47 82 00 00 01 3F
[32]90 0A 14 00 02 06 40 00
[40]0C 28 08 00

TB set (decoded):

TB 0:

TCTF:64
MAC SDU (160 bits):

[0]08 70 00 D4 C8 00 06 25
[8]2B F0 02 00 08 82 23 BF
[16]66 08 98 95

TB 1:

TCTF:64
MAC SDU (160 bits):

[0]0B 24 A5 47 82 00 00 01
[8]3F 90 0A 14 00 02 06 40
[16]00 0C 28 08

#### CPHY_SYNC_IND

PHY RRC @ 00:00:34.430

BTS unit: 1:1
Channel No: 0 Name: U_DPCH
CFN: 124

Message Details:

#### PHY_DATA_IND

PHY MAC @ 00:00:34.600

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 121

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 00 04 B0 C0 00 08 00
[8]00 51 1B 8D D0 6A 4C 66
[16]88 A2 C0 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 00 4B 0C 00 00 80 00
[8]05 11 B8 DD 06 A4 C6 68
[16]8A 2C

#### MAC_DATA_IND

MAC RLC @ 00:00:34.600

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 121

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 00 4B 0C 00 00 80 00
[8]05 11 B8 DD 06 A4 C6 68
[16]8A 2C

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:0
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]4B 0C 00 00 80 00 05 11
[8]B8 DD 06 A4 C6 68 8A 2C

#### PHY_DATA_IND

PHY MAC @ 00:00:34.610

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 122

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 00 88 30 34 80 01 80
[8]01 18 FC FC 0C C0 D5 C6
[16]28 48 C0 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 08 83 03 48 00 18 00
[8]11 8F CF C0 CC 0D 5C 62
[16]84 8C

#### MAC_DATA_IND

MAC RLC @ 00:00:34.610

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 122

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 08 83 03 48 00 18 00
[8]11 8F CF C0 CC 0D 5C 62
[16]84 8C

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:1
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]83 03 48 00 18 00 11 8F
[8]CF C0 CC 0D 5C 62 84 8C

#### PHY_DATA_IND

PHY MAC @ 00:00:34.620

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 123

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 01 50 BF E0 28 99 01
[8]00 05 55 55 55 55 55 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 15 0B FE 02 89 90 10
[8]00 55 55 55 55 55 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:00:34.620

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 123

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 15 0B FE 02 89 90 10
[8]00 55 55 55 55 55 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:2
Polling bit:1 (request a status report)
Length indicator 0 (octets):5
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (5 octets):

[0]02 89 90 10 00
Padding associated with length indicator 1 (9 octets):

[0]55 55 55 55 55 55 55 55
[8]55

#### MAC_DATA_REQ

RLC MAC @ 00:00:34.630

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 144

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:3

#### PHY_DATA_REQ

MAC PHY @ 00:00:34.630

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 144

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]10 20 03 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:00:34.630

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 124

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 00 01 58 21 D0 11 04
[8]00 81 72 A0 09 83 82 02
[16]FA 04 C0 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 00 15 82 1D 01 10 40
[8]08 17 2A 00 98 38 20 2F
[16]A0 4C

#### MAC_DATA_IND

MAC RLC @ 00:00:34.630

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 124

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 00 15 82 1D 01 10 40
[8]08 17 2A 00 98 38 20 2F
[16]A0 4C

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:0
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]15 82 1D 01 10 40 08 17
[8]2A 00 98 38 20 2F A0 4C

#### PHY_DATA_IND

PHY MAC @ 00:00:34.640

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 125

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 00 83 B2 A1 80 78 88
[8]00 00 82 85 8A F9 C1 19
[16]AA 15 10 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 08 3B 2A 18 07 88 80
[8]00 08 28 58 AF 9C 11 9A
[16]A1 51

#### MAC_DATA_IND

MAC RLC @ 00:00:34.640

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 125

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 08 3B 2A 18 07 88 80
[8]00 08 28 58 AF 9C 11 9A
[16]A1 51

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:1
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]3B 2A 18 07 88 80 00 08
[8]28 58 AF 9C 11 9A A1 51

#### RLC_AM_DATA_IND: rrcConnectionSetupComplete

RLC LLA @ 00:00:34.640

Channel No: 2 Name: DCCH

Message Details:

UL_DCCH_Message:

integrityCheckInfo: Omitted

message:

rrcConnectionSetupComplete:

rrc_TransactionIdentifier: 0

startList:

STARTList.element:

cn_DomainIdentity: ps_domain_CN_DomainIdentity [enum=1]

start_Value: 00000000000000000010

STARTList.element:

cn_DomainIdentity: cs_domain_CN_DomainIdentity [enum=0]

start_Value: 00000000000000000010

ue_RadioAccessCapability:

accessStratumReleaseIndicator: r99_AccessStratumReleaseIndicator [enum=0]

pdcp_Capability:

losslessSRNS_RelocationSupport: 0

supportForRfc2507:

notSupported: NULL

rlc_Capability:

totalRLC_AM_BufferSize: kb50_TotalRLC_AM_BufferSize [enum=2]

maximumRLC_WindowSize: mws2047_MaximumRLC_WindowSize [enum=0]

maximumAM_EntityNumber: am6_MaximumAM_EntityNumberRLC_Cap [enum=3]

transportChannelCapability:

dl_TransChCapability:

maxNoBitsReceived: b8960_MaxNoBits [enum=7]

maxConvCodeBitsReceived: b1280_MaxNoBits [enum=1]

turboDecodingSupport:

supported: b8960_MaxNoBits [enum=7]

maxSimultaneousTransChs: e8_MaxSimultaneousTransChsDL [enum=1]

maxSimultaneousCCTrCH_Count: 1

maxReceivedTransportBlocks: tb32_MaxTransportBlocksDL [enum=3]

maxNumberOfTFC: tfc128_MaxNumberOfTFC_DL [enum=5]

maxNumberOfTF: tf64_MaxNumberOfTF [enum=1]

ul_TransChCapability:

maxNoBitsTransmitted: b3840_MaxNoBits [enum=3]

maxConvCodeBitsTransmitted: b1280_MaxNoBits [enum=1]

turboEncodingSupport:

supported: b3840_MaxNoBits [enum=3]

maxSimultaneousTransChs: e8_MaxSimultaneousTransChsUL [enum=2]

modeSpecificInfo:

fdd: NULL

maxTransmittedBlocks: tb32_MaxTransportBlocksUL [enum=4]

maxNumberOfTFC: tfc64_MaxNumberOfTFC_UL [enum=5]

maxNumberOfTF: tf32_MaxNumberOfTF [enum=0]

rf_Capability:

fddRF_Capability:

ue_PowerClass: 4

txRxFrequencySeparation: mhz190_TxRxFrequencySeparation [enum=0]

tddRF_Capability: Omitted

physicalChannelCapability:

fddPhysChCapability:

downlinkPhysChCapability:

maxNoDPCH_PDSCH_Codes: 1

maxNoPhysChBitsReceived: b9600_MaxNoPhysChBitsReceived [enum=6]

supportForSF_512: 0

supportOfPDSCH: 0

simultaneousSCCPCH_DPCH_Reception:

notSupported: NULL

uplinkPhysChCapability:

maxNoDPDCH_BitsTransmitted: b4800_MaxNoDPDCH_BitsTransmitted [enum=3]

supportOfPCPCH: 0

tddPhysChCapability: Omitted

ue_MultiModeRAT_Capability:

multiRAT_CapabilityList:

supportOfGSM: 1

supportOfMulticarrier: 0

multiModeCapability: fdd_MultiModeCapability [enum=1]

securityCapability:

cipheringAlgorithmCap: 0000000000000011

integrityProtectionAlgorithmCap: 0000000000000010

ue_positioning_Capability:

standaloneLocMethodsSupported: 0

ue_BasedOTDOA_Supported: 0

networkAssistedGPS_Supported: noNetworkAssistedGPS_NetworkAssistedGPS_Supported [enum=3]

supportForUE_GPS_TimingOfCellFrames: 0

supportForIPDL: 0

measurementCapability:

downlinkCompressedMode:

fdd_Measurements: 1

tdd_Measurements: Omitted

gsm_Measurements:

gsm900: 1

dcs1800: 1

gsm1900: 1

multiCarrierMeasurements: 0

uplinkCompressedMode:

fdd_Measurements: 1

tdd_Measurements: Omitted

gsm_Measurements:

gsm900: 1

dcs1800: 1

gsm1900: 1

multiCarrierMeasurements: 0

ue_RATSpecificCapability:

InterRAT_UE_RadioAccessCapabilityList.element:

gsm:

gsm_Classmark2: 33035718A1

gsm_Classmark3: 60144C8080

v370NonCriticalExtensions: Omitted

Layer 3 SDU:

[0]4B 0C 00 00 80 00 05 11
[8]B8 DD 06 A4 C6 68 8A 2C
[16]83 03 48 00 18 00 11 8F
[24]CF C0 CC 0D 5C 62 84 8C
[32]02 89 90 10 00

#### RLC_AM_DATA_IND

LLA RRC @ 00:00:34.640

Channel ID: Rb2
Cell ID: -1

Message Details:

RLC_AM_DATA_IND:

cellId:-1

routingInfo:

rB_Identity:2

integrityResult:

integrityUsed (IntegrityStatus):i_pass

aM_message:

uL_DCCH_Message:

integrityCheckInfo: Omit

message: (UL_DCCH_MessageType)

rrcConnectionSetupComplete:

rrc_TransactionIdentifier:0

startList:

STARTSingle:

cn_DomainIdentity:ps_domain
start_Value:00000000000000000010

STARTSingle:

cn_DomainIdentity:cs_domain
start_Value:00000000000000000010

ue_RadioAccessCapability:

accessStratumReleaseIndicator:r99

pdcp_Capability:

losslessSRNS_RelocationSupport:false

supportForRfc2507:

notSupported:

rlc_Capability:

totalRLC_AM_BufferSize:kb50
maximumRLC_WindowSize:mws2047
maximumAM_EntityNumber (MaximumAM_EntityNumberRLC_Cap):am6

transportChannelCapability:

dl_TransChCapability:

maxNoBitsReceived (MaxNoBits):b8960
maxConvCodeBitsReceived (MaxNoBits):b1280

turboDecodingSupport: (TurboSupport)

supported (MaxNoBits):b8960

maxSimultaneousTransChs (MaxSimultaneousTransChsDL):e8
maxSimultaneousCCTrCH_Count:1
maxReceivedTransportBlocks (MaxTransportBlocksDL):tb32
maxNumberOfTFC (MaxNumberOfTFC_DL):tfc128
maxNumberOfTF:tf64

ul_TransChCapability:

maxNoBitsTransmitted (MaxNoBits):b3840
maxConvCodeBitsTransmitted (MaxNoBits):b1280

turboEncodingSupport: (TurboSupport)

supported (MaxNoBits):b3840

maxSimultaneousTransChs (MaxSimultaneousTransChsUL):e8

modeSpecificInfo:

fdd:

maxTransmittedBlocks (MaxTransportBlocksUL):tb32
maxNumberOfTFC (MaxNumberOfTFC_UL):tfc64
maxNumberOfTF:tf32

rf_Capability:

fddRF_Capability:

ue_PowerClass:4
txRxFrequencySeparation:mhz190

tddRF_Capability: Omit

physicalChannelCapability:

fddPhysChCapability:

downlinkPhysChCapability: (DL_PhysChCapabilityFDD)

maxNoDPCH_PDSCH_Codes:1
maxNoPhysChBitsReceived:b9600
supportForSF_512:false
supportOfPDSCH:false

simultaneousSCCPCH_DPCH_Reception:

notSupported:

uplinkPhysChCapability: (UL_PhysChCapabilityFDD)

maxNoDPDCH_BitsTransmitted:b4800
supportOfPCPCH:false

tddPhysChCapability: Omit

ue_MultiModeRAT_Capability:

multiRAT_CapabilityList: (MultiRAT_Capability)

supportOfGSM:true
supportOfMulticarrier:false

multiModeCapability:fdd

securityCapability:

cipheringAlgorithmCap:0000000000000011
integrityProtectionAlgorithmCap:0000000000000010

ue_positioning_Capability:

standaloneLocMethodsSupported:false
ue_BasedOTDOA_Supported:false
networkAssistedGPS_Supported:noNetworkAssistedGPS
supportForUE_GPS_TimingOfCellFrames:false
supportForIPDL:false

measurementCapability:

downlinkCompressedMode: (CompressedModeMeasCapability)

fdd_Measurements:true
tdd_Measurements: Omit

gsm_Measurements:

gsm900:true
dcs1800:true
gsm1900:true

multiCarrierMeasurements:false

uplinkCompressedMode: (CompressedModeMeasCapability)

fdd_Measurements:true
tdd_Measurements: Omit

gsm_Measurements:

gsm900:true
dcs1800:true
gsm1900:true

multiCarrierMeasurements:false

ue_RATSpecificCapability: (InterRAT_UE_RadioAccessCapabilityList)

InterRAT_UE_RadioAccessCapability:

gsm:

gsm_Classmark2:

[0]33 03 57 18 A1
gsm_Classmark3:

[0]60 14 4C 80 80

v370NonCriticalExtensions: Omit

#### PHY_DATA_IND

PHY MAC @ 00:00:34.650

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 126

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 01 51 7F E9 93 22 50
[8]CC 0B 8B 48 20 00 04 05
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 15 17 FE 99 32 25 0C
[8]C0 B8 B4 82 00 00 40 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:00:34.650

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 126

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 15 17 FE 99 32 25 0C
[8]C0 B8 B4 82 00 00 40 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:2
Polling bit:1 (request a status report)
Length indicator 0 (octets):11
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (11 octets):

[0]99 32 25 0C C0 B8 B4 82
[8]00 00 40
Padding associated with length indicator 1 (3 octets):

[0]55 55 55

#### RLC_AM_DATA_IND: initialDirectTransfer

RLC RRC @ 00:00:34.660

Channel No: 3 Name: DCCH

Message Details:

UL_DCCH_Message:

integrityCheckInfo: Omitted

message:

initialDirectTransfer:

cn_DomainIdentity: ps_domain_CN_DomainIdentity [enum=1]

intraDomainNasNodeSelector:

version:

release99:

cn_Type:

gsm_Map_IDNNS:

routingbasis:

localPTMSI:

routingparameter: 1000011101

enteredparameter: 0

nas_Message: 080102E54013070405F40987654300F1100001050B15F38233542A332644A198171690

measuredResultsOnRACH: Omitted

v3a0NonCriticalExtensions:

initialDirectTransfer_v3a0ext:

start_Value: 00000000000000000010

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]15 82 1D 01 10 40 08 17
[8]2A 00 98 38 20 2F A0 4C
[16]3B 2A 18 07 88 80 00 08
[24]28 58 AF 9C 11 9A A1 51
[32]99 32 25 0C C0 B8 B4 82
[40]00 00 40

#### RRC_DATA_IND: gmm:attachRequest

RRC NAS @ 00:00:34.660

Cell ID: -1

Message Details:

ATTACHREQUEST:

skipIndicator: 0000

gMMProtocolDiscriminator: 1000

msgType: 00000001

msNetworkCap:

iel: 02

value: E540

gprsCiphKeySeqNo:

spare1: 0

keySeq: 001

attachType:

for: 0

type: 011

drxParameter:

splitPGcycleCode: 00000111

cnDRXcoef: 0000

splitOnCCCH: 0

nonDRXtimer: 100

ptmsiORimsi:

iel: 05

iDigit1: 1111

oddEvenInd: 0

typeOfId: 100

otherDigits: 09876543

oldRAI:

plmn: 00F110

lac: 0001

rac: 05

msRadioAccessCap:

iel: 0B

value: 15F38233542A332644A198

oldPTMSI_Signature: Omitted

readyTimer:

iei: 00010111

unit: 000

value: 10110

tmsiStatus:

iei: 1001

spare3: 000

flag: 0

#### MAC_DATA_REQ

RLC MAC @ 00:00:34.660

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 147

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:3

#### PHY_DATA_REQ

MAC PHY @ 00:00:34.660

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 147

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 03 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### RRC_DATA_REQ: gmm:authenticationAndCipheringRequest

NAS RRC @ 00:00:34.680

Cell ID: -1

Message Details:

AUTHENTICATIONANDCIPHERINGREQUEST:

skipIndicator: 0000

gMMProtocolDiscriminator: 1000

msgType: 00010010

imeisvReq:

spare1: 0

value: 000

ciphAlgorithm:

spare1: 0

algorithm: 001

acRefNo:

value: 0011

forceToStandby:

spare: 0

value: 000

authRand:

iei: 00100001

randValue: 01010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101

gprsCiphKeySeqNo:

iei: 1000

spare1: 0

keySeq: 000

aUTN:

iei: 00101000

iel: 10

aUTN: 01100110000100010000000000110011001000101101110100000000000000000101010101000100011101110110011000010001000000000011001100100010

#### RLC_AM_DATA_REQ:downlinkDirectTransfer

RRC RLC @ 00:00:34.680

Channel No: 3 Name: DCCH

Message Details:

Opt1: 0

Opt2: 0

DL_DCCH_Message:

integrityCheckInfo: Omitted

message:

downlinkDirectTransfer:

r3:

downlinkDirectTransfer_r3:

rrc_TransactionIdentifier: 0

cn_DomainIdentity: ps_domain_CN_DomainIdentity [enum=1]

nas_Message: 0812013021555555555555555555555555555555558028106611003322DD00005544776611003322

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]14 20 4E 10 24 02 60 42
[8]AA AA AA AA AA AA AA AA
[16]AA AA AA AA AA AA AA AB
[24]00 50 20 CC 22 00 66 45
[32]BA 00 00 AA 88 EE CC 22
[40]00 66 44

#### MAC_DATA_REQ

RLC MAC @ 00:00:34.690

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 150

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 00 14 20 4E 10 24 02
[8]60 42 AA AA AA AA AA AA
[16]AA AA

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:0
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]14 20 4E 10 24 02 60 42
[8]AA AA AA AA AA AA AA AA

#### MAC_DATA_REQ

RLC MAC @ 00:00:34.690

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 150

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 08 AA AA AA AA AA AA
[8]AA AB 00 50 20 CC 22 00
[16]66 45

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:1
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]AA AA AA AA AA AA AA AB
[8]00 50 20 CC 22 00 66 45

#### MAC_DATA_REQ

RLC MAC @ 00:00:34.690

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 150

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 15 17 FE BA 00 00 AA
[8]88 EE CC 22 00 66 44 00
[16]00 00

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:2
Polling bit:1 (request a status report)
Length indicator 0 (octets):11
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (11 octets):

[0]BA 00 00 AA 88 EE CC 22
[8]00 66 44
Padding associated with length indicator 1 (3 octets):

[0]00 00 00

#### PHY_DATA_REQ

MAC PHY @ 00:00:34.690

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 150

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 00 01 42 04 E1 02 40
[8]26 04 2A AA AA AA AA AA
[16]AA AA A0 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 00 14 20 4E 10 24 02
[8]60 42 AA AA AA AA AA AA
[16]AA AA

#### PHY_DATA_REQ

MAC PHY @ 00:00:34.700

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 151

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 00 8A AA AA AA AA AA
[8]AA AA B0 05 02 0C C2 20
[16]06 64 50 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 08 AA AA AA AA AA AA
[8]AA AB 00 50 20 CC 22 00
[16]66 45

#### PHY_DATA_REQ

MAC PHY @ 00:00:34.710

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 152

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 01 51 7F EB A0 00 0A
[8]A8 8E EC C2 20 06 64 40
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 15 17 FE BA 00 00 AA
[8]88 EE CC 22 00 66 44 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:00:34.830

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 144

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 01 50 BF E0 28 99 01
[8]00 05 55 55 55 55 55 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 15 0B FE 02 89 90 10
[8]00 55 55 55 55 55 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:00:34.830

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 144

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 15 0B FE 02 89 90 10
[8]00 55 55 55 55 55 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:2
Polling bit:1 (request a status report)
Length indicator 0 (octets):5
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (5 octets):

[0]02 89 90 10 00
Padding associated with length indicator 1 (9 octets):

[0]55 55 55 55 55 55 55 55
[8]55

#### MAC_DATA_REQ

RLC MAC @ 00:00:34.840

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 165

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:3

#### PHY_DATA_REQ

MAC PHY @ 00:00:34.840

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 165

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]10 20 03 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:00:34.860

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 147

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 01 51 7F E9 93 22 50
[8]CC 0B 8B 48 20 00 04 05
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 15 17 FE 99 32 25 0C
[8]C0 B8 B4 82 00 00 40 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:00:34.860

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 147

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 15 17 FE 99 32 25 0C
[8]C0 B8 B4 82 00 00 40 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:2
Polling bit:1 (request a status report)
Length indicator 0 (octets):11
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (11 octets):

[0]99 32 25 0C C0 B8 B4 82
[8]00 00 40
Padding associated with length indicator 1 (3 octets):

[0]55 55 55

#### MAC_DATA_REQ

RLC MAC @ 00:00:34.870

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 168

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:3

#### PHY_DATA_REQ

MAC PHY @ 00:00:34.870

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 168

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 03 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### MAC_DATA_REQ

RLC MAC @ 00:00:34.890

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 170

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 15 17 FE BA 00 00 AA
[8]88 EE CC 22 00 66 44 00
[16]00 00

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:2
Polling bit:1 (request a status report)
Length indicator 0 (octets):11
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (11 octets):

[0]BA 00 00 AA 88 EE CC 22
[8]00 66 44
Padding associated with length indicator 1 (3 octets):

[0]00 00 00

#### PHY_DATA_REQ

MAC PHY @ 00:00:34.890

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 170

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 01 51 7F EB A0 00 0A
[8]A8 8E EC C2 20 06 64 40
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 15 17 FE BA 00 00 AA
[8]88 EE CC 22 00 66 44 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:00:34.940

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 155

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 03 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### MAC_DATA_IND

MAC RLC @ 00:00:34.940

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 155

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:3

#### PHY_DATA_IND

PHY MAC @ 00:00:35.090

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 170

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 01 86 C8 06 84 09 81
[8]91 2A A2 3B B3 14 82 08
[16]80 19 90 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 18 6C 80 68 40 98 19
[8]12 AA 23 BB 31 48 20 88
[16]01 99

#### MAC_DATA_IND

MAC RLC @ 00:00:35.090

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 170

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 18 6C 80 68 40 98 19
[8]12 AA 23 BB 31 48 20 88
[16]01 99

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:3
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]6C 80 68 40 98 19 12 AA
[8]23 BB 31 48 20 88 01 99

#### PHY_DATA_IND

PHY MAC @ 00:00:35.100

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 171

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 02 50 3F E1 05 55 55
[8]55 55 55 55 55 55 55 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 25 03 FE 10 55 55 55
[8]55 55 55 55 55 55 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:00:35.100

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 171

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 25 03 FE 10 55 55 55
[8]55 55 55 55 55 55 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:4
Polling bit:1 (request a status report)
Length indicator 0 (octets):1
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (1 octets):

[0]10
Padding associated with length indicator 1 (13 octets):

[0]55 55 55 55 55 55 55 55
[8]55 55 55 55 55

#### RLC_AM_DATA_IND: uplinkDirectTransfer

RLC RRC @ 00:00:35.110

Channel No: 3 Name: DCCH

Message Details:

UL_DCCH_Message:

integrityCheckInfo: Omitted

message:

uplinkDirectTransfer:

cn_DomainIdentity: ps_domain_CN_DomainIdentity [enum=1]

nas_Message: 0813032255447766290411003322

measuredResultsOnRACH: Omitted

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]6C 80 68 40 98 19 12 AA
[8]23 BB 31 48 20 88 01 99
[16]10

#### RRC_DATA_IND: gmm:authenticationAndCipheringResponse

RRC NAS @ 00:00:35.110

Cell ID: -1

Message Details:

AUTHENTICATIONANDCIPHERINGRESPONSE:

skipIndicator: 0000

gMMProtocolDiscriminator: 1000

msgType: 00010011

spare4: 0000

acRefNo:

value: 0011

authRsp:

iei: 00100010

value: 01010101010001000111011101100110

imeisv: Omitted

authRspExt:

iei: 00101001

iel: 04

rES: 00010001000000000011001100100010

#### CRLC_SecurityMode_Config_REQ

RRC LLA @ 00:00:35.110

Cell ID: -1

Message Details:

CRLC_SecurityMode_Config_REQ:

cellId:-1

rlcSecurityInfo: (SecurityInfo)

cn_DomainIdentity:ps_domain
startValue (START_Value):00000000000000000000
cipheringKey: Omit
integrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
gsmCipheringKey: Omit

#### CRLC_SecurityMode_Config_REQ

RRC RLC @ 00:00:35.110

Message Details:

cellIdentity: 1

rlcSecurityInfo:

cn_DomainIdentity: ps_domain_CN_DomainIdentity

startValue: 00000000000000000000

cipheringKey: Omitted

integrityKey: 01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100

#### MAC_DATA_REQ

RLC MAC @ 00:00:35.110

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 192

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 50 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:5

#### PHY_DATA_REQ

MAC PHY @ 00:00:35.110

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 192

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 05 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 50 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### CRLC_SecurityMode_Config_CNF

LLA RRC @ 00:00:35.130

Cell ID: -1

Message Details:

CRLC_SecurityMode_Config_CNF:

cellId:-1

#### CRLC_SetRRC_MessageSN_REQ

RRC LLA @ 00:00:35.130

Channel ID: Rb0
Cell ID: 0

Message Details:

CRLC_SetRRC_MessageSN_REQ:

cellId:0

routingInfo:

rB_Identity:0

count_I_LSB_UL (RRC_SequenceNumber): Omit
count_I_LSB_DL (RRC_SequenceNumber):0

#### CRLC_SetRRC_MessageSN_CNF

LLA RRC @ 00:00:35.140

Channel ID: Rb0
Cell ID: 0

Message Details:

CRLC_SetRRC_MessageSN_CNF:

cellId:0

routingInfo:

rB_Identity:0

#### CRLC_SetRRC_MessageSN_REQ

RRC LLA @ 00:00:35.140

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_REQ:

cellId:-1

routingInfo:

rB_Identity:1

count_I_LSB_UL (RRC_SequenceNumber): Omit
count_I_LSB_DL (RRC_SequenceNumber):0

#### PHY_DATA_IND

PHY MAC @ 00:00:35.150

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 176

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 03 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### MAC_DATA_IND

MAC RLC @ 00:00:35.150

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 176

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:3

#### CRLC_SetRRC_MessageSN_CNF

LLA RRC @ 00:00:35.160

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_CNF:

cellId:-1

routingInfo:

rB_Identity:1

#### CRLC_SetRRC_MessageSN_REQ

RRC LLA @ 00:00:35.160

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_REQ:

cellId:-1

routingInfo:

rB_Identity:2

count_I_LSB_UL (RRC_SequenceNumber): Omit
count_I_LSB_DL (RRC_SequenceNumber):0

#### CRLC_SetRRC_MessageSN_CNF

LLA RRC @ 00:00:35.180

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_CNF:

cellId:-1

routingInfo:

rB_Identity:2

#### CRLC_SetRRC_MessageSN_REQ

RRC LLA @ 00:00:35.180

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_REQ:

cellId:-1

routingInfo:

rB_Identity:3

count_I_LSB_UL (RRC_SequenceNumber): Omit
count_I_LSB_DL (RRC_SequenceNumber):0

#### CRLC_SetRRC_MessageSN_CNF

LLA RRC @ 00:00:35.190

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_CNF:

cellId:-1

routingInfo:

rB_Identity:3

#### CRLC_SetRRC_MessageSN_REQ

RRC LLA @ 00:00:35.190

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_REQ:

cellId:-1

routingInfo:

rB_Identity:4

count_I_LSB_UL (RRC_SequenceNumber): Omit
count_I_LSB_DL (RRC_SequenceNumber):0

#### CRLC_SetRRC_MessageSN_CNF

LLA RRC @ 00:00:35.210

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_CNF:

cellId:-1

routingInfo:

rB_Identity:4

#### CRLC_Integrity_Activate_REQ

RRC LLA @ 00:00:35.210

Cell ID: -1

Message Details:

CRLC_Integrity_Activate_REQ:

cellId:-1
cn_DomainIdentity:ps_domain

integrityActivationInfo:

integrityProtectionModeInfo:

integrityProtectionModeCommand:

startIntegrityProtection:

integrityProtInitNumber:00001111000011110000111100001111

integrityProtectionAlgorithm:uia1

#### CRLC_Integrity_Activate_REQ

RRC RLC @ 00:00:35.210

Message Details:

cellIdentity: 1

integrityActivationInfo:

integrityProtectionModeInfo:

integrityProtectionModeCommand:

startIntegrityProtection:

integrityProtInitNumber: 00001111000011110000111100001111

#### CRLC_Integrity_Activate_CNF

LLA RRC @ 00:00:35.220

Cell ID: -1

Message Details:

CRLC_Integrity_Activate_CNF:

cellId:-1

#### CRLC_Integrity_Activate_REQ

RRC LLA @ 00:00:35.220

Cell ID: -1

Message Details:

CRLC_Integrity_Activate_REQ:

cellId:-1
cn_DomainIdentity:ps_domain

integrityActivationInfo:

ul_IntegProtActivationInfo: (IntegrityProtActivationInfoList)

SS_IntegrityProtActivationTimeInfo:

rb_Identity:2
rrc_MessageSequenceNumber:0

#### CRLC_Integrity_Activate_REQ

RRC RLC @ 00:00:35.220

Message Details:

cellIdentity: 1

integrityActivationInfo:

ul_IntegrityProtActivationInfo:

rrc_MessageSequenceNumberList:

RRC_MessageSequenceNumberList.element: -2

RRC_MessageSequenceNumberList.element: -2

RRC_MessageSequenceNumberList.element: 0

RRC_MessageSequenceNumberList.element: -2

RRC_MessageSequenceNumberList.element: -2

#### CMAC Integrity Check Request

RRC MAC @ 00:00:35.240

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000001
Data:

[0]00 00 00 01
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:1 (RNC to UE)
Message Length (bits):128
Message:

[0]80 00 00 01 04 06 00 01
[8]80 01 41 E1 E1 E1 F0 18

#### CMAC Integrity Check Result

MAC RRC @ 00:00:35.240

Message Details:

Integrity Check Result:

MAC-I:00011001111101010100011100101111
Data:

[0]19 F5 47 2F

#### CRLC_Integrity_Activate_CNF

LLA RRC @ 00:00:35.240

Cell ID: -1

Message Details:

CRLC_Integrity_Activate_CNF:

cellId:-1

#### RLC_AM_DATA_REQ

RRC LLA @ 00:00:35.240

Channel ID: Rb2
Cell ID: -1

Message Details:

RLC_AM_DATA_REQ:

cellId:-1

routingInfo:

rB_Identity:2

confirmationRequest: (AmConfirmationRequest)

noConfirmationRequest:

aM_message:

dL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode:00000000000000000000000000000000
rrc_MessageSequenceNumber:0

message: (DL_DCCH_MessageType)

securityModeCommand:

r3:

securityModeCommand_r3: (SecurityModeCommand_r3_IEs)

rrc_TransactionIdentifier:0

securityCapability:

cipheringAlgorithmCap:0000000000000011
integrityProtectionAlgorithmCap:0000000000000010

cipheringModeInfo: Omit

integrityProtectionModeInfo:

integrityProtectionModeCommand:

startIntegrityProtection:

integrityProtInitNumber:00001111000011110000111100001111

integrityProtectionAlgorithm:uia1

cn_DomainIdentity:ps_domain

ue_SystemSpecificSecurityCap: (InterRAT_UE_SecurityCapList)

InterRAT_UE_SecurityCapability:

gsm:

gsmSecurityCapability:0000011

laterNonCriticalExtensions: Omit

#### RLC_AM_DATA_REQ: securityModeCommand

LLA RLC @ 00:00:35.240

Channel No: 2 Name: DCCH

Message Details:

DL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode: 00011001111101010100011100101111

rrc_MessageSequenceNumber: 1

message:

securityModeCommand:

r3:

securityModeCommand_r3:

rrc_TransactionIdentifier: 0

securityCapability:

cipheringAlgorithmCap: 0000000000000011

integrityProtectionAlgorithmCap: 0000000000000010

cipheringModeInfo: Omitted

integrityProtectionModeInfo:

integrityProtectionModeCommand:

startIntegrityProtection:

integrityProtInitNumber: 00001111000011110000111100001111

integrityProtectionAlgorithm: uia1_IntegrityProtectionAlgorithm [enum=0]

cn_DomainIdentity: ps_domain_CN_DomainIdentity [enum=1]

ue_SystemSpecificSecurityCap:

InterRAT_UE_SecurityCapList.element:

gsm:

gsmSecurityCapability: 0000011

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]8C FA A3 97 8C 06 00 01
[8]80 01 41 E1 E1 E1 F0 18

#### MAC_DATA_REQ

RLC MAC @ 00:00:35.250

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 206

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 00 8C FA A3 97 8C 06
[8]00 01 80 01 41 E1 E1 E1
[16]F0 18

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:0
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]8C FA A3 97 8C 06 00 01
[8]80 01 41 E1 E1 E1 F0 18

#### MAC_DATA_REQ

RLC MAC @ 00:00:35.250

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 206

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 0D 01 FE 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:1
Polling bit:1 (request a status report)
Length indicator 0 (octets):0 (the previous RLC PDU was exactly filled by the last segment of an RLC SDU)
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (0 octets):

Padding associated with length indicator 1 (14 octets):

[0]00 00 00 00 00 00 00 00
[8]00 00 00 00 00 00

#### PHY_DATA_REQ

MAC PHY @ 00:00:35.250

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 206

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 00 08 CF AA 39 78 C0
[8]60 00 18 00 14 1E 1E 1E
[16]1F 01 80 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 00 8C FA A3 97 8C 06
[8]00 01 80 01 41 E1 E1 E1
[16]F0 18

#### PHY_DATA_REQ

MAC PHY @ 00:00:35.260

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 207

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 00 D0 1F E0 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 0D 01 FE 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:00:35.310

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 192

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 02 50 3F E1 05 55 55
[8]55 55 55 55 55 55 55 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 25 03 FE 10 55 55 55
[8]55 55 55 55 55 55 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:00:35.310

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 192

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 25 03 FE 10 55 55 55
[8]55 55 55 55 55 55 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:4
Polling bit:1 (request a status report)
Length indicator 0 (octets):1
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (1 octets):

[0]10
Padding associated with length indicator 1 (13 octets):

[0]55 55 55 55 55 55 55 55
[8]55 55 55 55 55

#### MAC_DATA_REQ

RLC MAC @ 00:00:35.320

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 213

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 50 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:5

#### PHY_DATA_REQ

MAC PHY @ 00:00:35.320

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 213

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 05 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 50 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### MAC_DATA_REQ

RLC MAC @ 00:00:35.450

Category: Configuration
BTS unit: 1:?
Channel No: 2 Name: DCCH
CFN: 226

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 0D 01 FE 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:1
Polling bit:1 (request a status report)
Length indicator 0 (octets):0 (the previous RLC PDU was exactly filled by the last segment of an RLC SDU)
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (0 octets):

Padding associated with length indicator 1 (14 octets):

[0]00 00 00 00 00 00 00 00
[8]00 00 00 00 00 00

#### PHY_DATA_REQ

MAC PHY @ 00:00:35.450

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 226

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 00 D0 1F E0 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 0D 01 FE 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:00:35.490

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 210

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]10 20 02 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]02 00 20 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### MAC_DATA_IND

MAC RLC @ 00:00:35.490

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 210

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 20 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:2

#### PHY_DATA_IND

PHY MAC @ 00:00:35.500

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 211

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 01 D1 3F EC 59 1B E7
[8]10 D2 10 00 00 05 55 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 1D 13 FE C5 91 BE 71
[8]0D 21 00 00 00 55 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:00:35.500

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 211

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 1D 13 FE C5 91 BE 71
[8]0D 21 00 00 00 55 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:3
Polling bit:1 (request a status report)
Length indicator 0 (octets):9
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (9 octets):

[0]C5 91 BE 71 0D 21 00 00
[8]00
Padding associated with length indicator 1 (5 octets):

[0]55 55 55 55 55

#### MAC_DATA_REQ

RLC MAC @ 00:00:35.510

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 232

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 40 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:4

#### PHY_DATA_REQ

MAC PHY @ 00:00:35.510

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 232

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]10 20 04 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]02 00 40 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### CMAC Integrity Check Request

RRC MAC @ 00:00:35.540

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000001
Data:

[0]00 00 00 01
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:0 (UE to RNC)
Message Length (bits):72
Message:

[0]80 00 00 01 05 21 00 00
[8]00

#### RLC_AM_DATA_IND: securityModeComplete

RLC LLA @ 00:00:35.540

Channel No: 2 Name: DCCH

Message Details:

UL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode: 10001011001000110111110011100010

rrc_MessageSequenceNumber: 1

message:

securityModeComplete:

rrc_TransactionIdentifier: 0

ul_IntegProtActivationInfo:

rrc_MessageSequenceNumberList:

RRC_MessageSequenceNumberList.element: 0

RRC_MessageSequenceNumberList.element: 0

RRC_MessageSequenceNumberList.element: 0

RRC_MessageSequenceNumberList.element: 0

RRC_MessageSequenceNumberList.element: 0

rb_UL_CiphActivationTimeInfo: Omitted

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]C5 91 BE 71 0D 21 00 00
[8]00

#### CMAC Integrity Check Result

MAC RRC @ 00:00:35.540

Message Details:

Integrity Check Result:

MAC-I:10001011001000110111110011100010
Data:

[0]8B 23 7C E2

#### RLC_AM_DATA_IND

LLA RRC @ 00:00:35.540

Channel ID: Rb2
Cell ID: -1

Message Details:

RLC_AM_DATA_IND:

cellId:-1

routingInfo:

rB_Identity:2

integrityResult:

integrityUsed (IntegrityStatus):i_pass

aM_message:

uL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode:10001011001000110111110011100010
rrc_MessageSequenceNumber:1

message: (UL_DCCH_MessageType)

securityModeComplete:

rrc_TransactionIdentifier:0

ul_IntegProtActivationInfo: (IntegrityProtActivationInfo)

rrc_MessageSequenceNumberList:

RRC_MessageSequenceNumber:0
RRC_MessageSequenceNumber:0
RRC_MessageSequenceNumber:0
RRC_MessageSequenceNumber:0
RRC_MessageSequenceNumber:0

rb_UL_CiphActivationTimeInfo: (RB_ActivationTimeInfoList) Omit

laterNonCriticalExtensions: Omit

#### CRLC_Integrity_Activate_REQ

RRC LLA @ 00:00:35.540

Cell ID: -1

Message Details:

CRLC_Integrity_Activate_REQ:

cellId:-1
cn_DomainIdentity:ps_domain

integrityActivationInfo:

ul_IntegProtActivationInfo: (IntegrityProtActivationInfoList)

SS_IntegrityProtActivationTimeInfo:

rb_Identity:0
rrc_MessageSequenceNumber:0

SS_IntegrityProtActivationTimeInfo:

rb_Identity:1
rrc_MessageSequenceNumber:0

SS_IntegrityProtActivationTimeInfo:

rb_Identity:3
rrc_MessageSequenceNumber:0

SS_IntegrityProtActivationTimeInfo:

rb_Identity:4
rrc_MessageSequenceNumber:0

#### CRLC_Integrity_Activate_REQ

RRC RLC @ 00:00:35.540

Message Details:

cellIdentity: 1

integrityActivationInfo:

ul_IntegrityProtActivationInfo:

rrc_MessageSequenceNumberList:

RRC_MessageSequenceNumberList.element: 0

RRC_MessageSequenceNumberList.element: 0

RRC_MessageSequenceNumberList.element: -2

RRC_MessageSequenceNumberList.element: 0

RRC_MessageSequenceNumberList.element: 0

#### CMAC Integrity Check Request

RRC MAC @ 00:00:35.550

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000001
Data:

[0]00 00 00 01
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:1 (RNC to UE)
Message Length (bits):296
Message:

[0]80 00 00 01 81 42 03 81
[8]00 40 7C 00 80 1E 22 00
[16]00 20 A3 35 62 46 83 00
[24]BE 82 46 8A CF 04 60 BE
[32]82 24 46 68 80

#### CMAC Integrity Check Result

MAC RRC @ 00:00:35.550

Message Details:

Integrity Check Result:

MAC-I:10100000000110000010111001100001
Data:

[0]A0 18 2E 61

#### CRLC_Integrity_Activate_CNF

LLA RRC @ 00:00:35.550

Cell ID: -1

Message Details:

CRLC_Integrity_Activate_CNF:

cellId:-1

#### RRC_DATA_REQ: gmm:attachAccept

NAS RRC @ 00:00:35.550

Cell ID: -1

Message Details:

ATTACHACCEPT:

skipIndicator: 0000

gMMProtocolDiscriminator: 1000

msgType: 00000010

forceToStandby:

spare: 0

value: 000

attachResult:

spare: 0

result: 011

periodicRAupdateTimer:

unit: 111

value: 00000

spare: 0000

radioPrioSMS:

spare: 0

value: 100

rai:

plmn: 00F110

lac: 0001

rac: 05

ptmsiSignature:

iei: 00011001

value: AB1234

negReadyTimer: Omitted

allocatedPTMSI:

iei: 00011000

iel: 05

iDigit1: 1111

oddEvenInd: 0

typeOfId: 100

otherDigits: 12345678

msIdentity:

iei: 00100011

iel: 05

iDigit1: 1111

oddEvenInd: 0

typeOfId: 100

otherDigits: 11223344

gmmCause: Omitted

t3302Value: Omitted

cellNotification: Omitted

equivalentPLMN: Omitted

#### RLC_AM_DATA_REQ:downlinkDirectTransfer

RRC RLC @ 00:00:35.550

Channel No: 3 Name: DCCH

Message Details:

Opt1: 0

Opt2: 0

DL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode: 10100000000110000010111001100001

rrc_MessageSequenceNumber: 1

message:

downlinkDirectTransfer:

r3:

downlinkDirectTransfer_r3:

rrc_TransactionIdentifier: 0

cn_DomainIdentity: ps_domain_CN_DomainIdentity [enum=1]

nas_Message: 080203E00400F11000010519AB12341805F4123456782305F411223344

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]D0 0C 17 30 89 42 03 81
[8]00 40 7C 00 80 1E 22 00
[16]00 20 A3 35 62 46 83 00
[24]BE 82 46 8A CF 04 60 BE
[32]82 24 46 68 80

#### MAC_DATA_REQ

RLC MAC @ 00:00:35.560

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 237

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 18 D0 0C 17 30 89 42
[8]03 81 00 40 7C 00 80 1E
[16]22 00

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:3
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]D0 0C 17 30 89 42 03 81
[8]00 40 7C 00 80 1E 22 00

#### MAC_DATA_REQ

RLC MAC @ 00:00:35.560

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 237

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 20 00 20 A3 35 62 46
[8]83 00 BE 82 46 8A CF 04
[16]60 BE

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:4
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]00 20 A3 35 62 46 83 00
[8]BE 82 46 8A CF 04 60 BE

#### MAC_DATA_REQ

RLC MAC @ 00:00:35.560

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 237

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 2D 0B FE 82 24 46 68
[8]80 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:5
Polling bit:1 (request a status report)
Length indicator 0 (octets):5
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (5 octets):

[0]82 24 46 68 80
Padding associated with length indicator 1 (9 octets):

[0]00 00 00 00 00 00 00 00
[8]00

#### PHY_DATA_REQ

MAC PHY @ 00:00:35.560

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 237

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 01 8D 00 C1 73 08 94
[8]20 38 10 04 07 C0 08 01
[16]E2 20 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 18 D0 0C 17 30 89 42
[8]03 81 00 40 7C 00 80 1E
[16]22 00

#### PHY_DATA_REQ

MAC PHY @ 00:00:35.570

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 238

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 02 00 02 0A 33 56 24
[8]68 30 0B E8 24 68 AC F0
[16]46 0B E0 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 20 00 20 A3 35 62 46
[8]83 00 BE 82 46 8A CF 04
[16]60 BE

#### PHY_DATA_REQ

MAC PHY @ 00:00:35.580

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 239

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 02 D0 BF E8 22 44 66
[8]88 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 2D 0B FE 82 24 46 68
[8]80 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:00:35.700

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 231

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]10 20 02 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]02 00 20 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### MAC_DATA_IND

MAC RLC @ 00:00:35.700

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 231

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 20 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:2

#### PHY_DATA_IND

PHY MAC @ 00:00:35.710

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 232

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 01 D1 3F EC 59 1B E7
[8]10 D2 10 00 00 05 55 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 1D 13 FE C5 91 BE 71
[8]0D 21 00 00 00 55 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:00:35.710

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 232

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 1D 13 FE C5 91 BE 71
[8]0D 21 00 00 00 55 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:3
Polling bit:1 (request a status report)
Length indicator 0 (octets):9
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (9 octets):

[0]C5 91 BE 71 0D 21 00 00
[8]00
Padding associated with length indicator 1 (5 octets):

[0]55 55 55 55 55

#### MAC_DATA_REQ

RLC MAC @ 00:00:35.720

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 253

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 40 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:4

#### PHY_DATA_REQ

MAC PHY @ 00:00:35.720

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 253

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]10 20 04 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]02 00 40 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### MAC_DATA_REQ

RLC MAC @ 00:00:35.760

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 1

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 2D 0B FE 82 24 46 68
[8]80 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:5
Polling bit:1 (request a status report)
Length indicator 0 (octets):5
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (5 octets):

[0]82 24 46 68 80
Padding associated with length indicator 1 (9 octets):

[0]00 00 00 00 00 00 00 00
[8]00

#### PHY_DATA_REQ

MAC PHY @ 00:00:35.760

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 1

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 02 D0 BF E8 22 44 66
[8]88 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 2D 0B FE 82 24 46 68
[8]80 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:00:35.810

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 242

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 06 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 60 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### MAC_DATA_IND

MAC RLC @ 00:00:35.810

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 242

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 60 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:6

#### PHY_DATA_IND

PHY MAC @ 00:00:35.820

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 243

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 02 D1 5F ED 6F 6F 71
[8]E0 EC 80 08 40 18 05 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 2D 15 FE D6 F6 F7 1E
[8]0E C8 00 84 01 80 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:00:35.820

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 243

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 2D 15 FE D6 F6 F7 1E
[8]0E C8 00 84 01 80 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:5
Polling bit:1 (request a status report)
Length indicator 0 (octets):10
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (10 octets):

[0]D6 F6 F7 1E 0E C8 00 84
[8]01 80
Padding associated with length indicator 1 (4 octets):

[0]55 55 55 55

#### RLC_AM_DATA_IND: uplinkDirectTransfer

RLC RRC @ 00:00:35.830

Channel No: 3 Name: DCCH

Message Details:

UL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode: 10101101111011011110111000111100

rrc_MessageSequenceNumber: 1

message:

uplinkDirectTransfer:

cn_DomainIdentity: ps_domain_CN_DomainIdentity [enum=1]

nas_Message: 0803

measuredResultsOnRACH: Omitted

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]D6 F6 F7 1E 0E C8 00 84
[8]01 80

#### RRC_DATA_IND: gmm:attachComplete

RRC NAS @ 00:00:35.830

Cell ID: -1

Message Details:

ATTACHCOMPLETE:

skipIndicator: 0000

gMMProtocolDiscriminator: 1000

msgType: 00000011

#### MAC_DATA_REQ

RLC MAC @ 00:00:35.830

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 8

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 60 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:6

#### PHY_DATA_REQ

MAC PHY @ 00:00:35.830

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 8

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 06 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 60 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### CMAC Integrity Check Request

RRC MAC @ 00:00:35.850

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000001
Data:

[0]00 00 00 01
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:0 (UE to RNC)
Message Length (bits):80
Message:

[0]80 00 00 01 86 C8 00 84
[8]01 80

#### CMAC Integrity Check Result

MAC RRC @ 00:00:35.850

Message Details:

Integrity Check Result:

MAC-I:10101101111011011110111000111100
Data:

[0]AD ED EE 3C

#### PHY_DATA_IND

PHY MAC @ 00:00:36.020

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 7

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 06 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 60 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### MAC_DATA_IND

MAC RLC @ 00:00:36.020

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 7

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 60 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:6

#### PHY_DATA_IND

PHY MAC @ 00:00:36.030

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 8

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 02 D1 5F ED 6F 6F 71
[8]E0 EC 80 08 40 18 05 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 2D 15 FE D6 F6 F7 1E
[8]0E C8 00 84 01 80 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:00:36.030

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 8

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 2D 15 FE D6 F6 F7 1E
[8]0E C8 00 84 01 80 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:5
Polling bit:1 (request a status report)
Length indicator 0 (octets):10
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (10 octets):

[0]D6 F6 F7 1E 0E C8 00 84
[8]01 80
Padding associated with length indicator 1 (4 octets):

[0]55 55 55 55

#### MAC_DATA_REQ

RLC MAC @ 00:00:36.040

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 29

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 60 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:6

#### PHY_DATA_REQ

MAC PHY @ 00:00:36.040

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 29

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 06 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 60 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### CMAC Integrity Check Request

RRC MAC @ 00:00:36.860

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000001
Data:

[0]00 00 00 01
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:1 (RNC to UE)
Message Length (bits):56
Message:

[0]80 00 00 00 83 C8 00

#### CMAC Integrity Check Result

MAC RRC @ 00:00:36.860

Message Details:

Integrity Check Result:

MAC-I:11101100100111000001011111010011
Data:

[0]EC 9C 17 D3

#### RLC_UM_DATA_REQ

RRC LLA @ 00:00:36.860

Channel ID: Rb1
Cell ID: -1

Message Details:

RLC_UM_DATA_REQ:

cellId:-1

routingInfo:

rB_Identity:1

uM_message:

dL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode:00000000000000000000000000000000
rrc_MessageSequenceNumber:0

message: (DL_DCCH_MessageType)

rrcConnectionRelease:

r3:

rrcConnectionRelease_r3: (RRCConnectionRelease_r3_IEs)

rrc_TransactionIdentifier:0
n_308:1
releaseCause:normalEvent

rplmn_information: Omit

laterNonCriticalExtensions: Omit

specialLI:false

#### RLC_UM_DATA_REQ: rrcConnectionRelease

LLA RLC @ 00:00:36.860

Channel No: 1 Name: DCCH

Message Details:

DL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode: 11101100100111000001011111010011

rrc_MessageSequenceNumber: 1

message:

rrcConnectionRelease:

r3:

rrcConnectionRelease_r3:

rrc_TransactionIdentifier: 0

n_308: 1

releaseCause: normalEvent_ReleaseCause [enum=0]

rplmn_information: Omitted

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]F6 4E 0B E9 8B C8 00

#### MAC_DATA_REQ

RLC MAC @ 00:00:36.870

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 112

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]01 0F FE F6 4E 0B E9 8B
[8]C8 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

Sequence number:0
Length indicator 0 (octets):7
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (7 octets):

[0]F6 4E 0B E9 8B C8 00
Padding associated with length indicator 1 (8 octets):

[0]00 00 00 00 00 00 00 00

#### PHY_DATA_REQ

MAC PHY @ 00:00:36.870

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 112

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]00 10 FF EF 64 E0 BE 98
[8]BC 80 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:0
MAC SDU (144 bits):

[0]01 0F FE F6 4E 0B E9 8B
[8]C8 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:00:37.110

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 116

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]00 10 DF EF BF 16 16 70
[8]C4 05 55 55 55 55 55 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:0
MAC SDU (144 bits):

[0]01 0D FE FB F1 61 67 0C
[8]40 55 55 55 55 55 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:00:37.110

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 116

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]01 0D FE FB F1 61 67 0C
[8]40 55 55 55 55 55 55 55
[16]55 55

RLC PDU (decoded):

Sequence number:0
Length indicator 0 (octets):6
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (6 octets):

[0]FB F1 61 67 0C 40
Padding associated with length indicator 1 (9 octets):

[0]55 55 55 55 55 55 55 55
[8]55

#### CMAC Integrity Check Request

RRC MAC @ 00:00:37.130

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000001
Data:

[0]00 00 00 01
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:0 (UE to RNC)
Message Length (bits):48
Message:

[0]80 00 00 00 84 40

#### RLC_UM_DATA_IND: rrcConnectionReleaseComplete

RLC LLA @ 00:00:37.130

Channel No: 1 Name: DCCH

Message Details:

UL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode: 11110111111000101100001011001110

rrc_MessageSequenceNumber: 1

message:

rrcConnectionReleaseComplete:

rrc_TransactionIdentifier: 0

errorIndication: Omitted

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]FB F1 61 67 0C 40

#### CMAC Integrity Check Result

MAC RRC @ 00:00:37.130

Message Details:

Integrity Check Result:

MAC-I:11110111111000101100001011001110
Data:

[0]F7 E2 C2 CE

#### RLC_UM_DATA_IND

LLA RRC @ 00:00:37.130

Channel ID: Rb1
Cell ID: -1

Message Details:

RLC_UM_DATA_IND:

cellId:-1

routingInfo:

rB_Identity:1

integrityResult:

integrityUsed (IntegrityStatus):i_pass

uM_message:

uL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode:11110111111000101100001011001110
rrc_MessageSequenceNumber:1

message: (UL_DCCH_MessageType)

rrcConnectionReleaseComplete:

rrc_TransactionIdentifier:0

errorIndication: (FailureCauseWithProtErr) Omit

laterNonCriticalExtensions: Omit

#### PHY_DATA_IND

PHY MAC @ 00:00:37.270

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 132

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]00 30 DF ED CD 18 3E 01
[8]44 05 55 55 55 55 55 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:0
MAC SDU (144 bits):

[0]03 0D FE DC D1 83 E0 14
[8]40 55 55 55 55 55 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:00:37.270

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 132

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]03 0D FE DC D1 83 E0 14
[8]40 55 55 55 55 55 55 55
[16]55 55

RLC PDU (decoded):

Sequence number:1
Length indicator 0 (octets):6
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (6 octets):

[0]DC D1 83 E0 14 40
Padding associated with length indicator 1 (9 octets):

[0]55 55 55 55 55 55 55 55
[8]55

#### CMAC Integrity Check Request

RRC MAC @ 00:00:37.300

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000010
Data:

[0]00 00 00 02
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:0 (UE to RNC)
Message Length (bits):48
Message:

[0]80 00 00 00 84 40

#### RLC_UM_DATA_IND: rrcConnectionReleaseComplete

RLC LLA @ 00:00:37.300

Channel No: 1 Name: DCCH

Message Details:

UL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode: 10111001101000110000011111000000

rrc_MessageSequenceNumber: 2

message:

rrcConnectionReleaseComplete:

rrc_TransactionIdentifier: 0

errorIndication: Omitted

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]DC D1 83 E0 14 40

#### CMAC Integrity Check Result

MAC RRC @ 00:00:37.300

Message Details:

Integrity Check Result:

MAC-I:10111001101000110000011111000000
Data:

[0]B9 A3 07 C0

#### RLC_UM_DATA_IND

LLA RRC @ 00:00:37.300

Channel ID: Rb1
Cell ID: -1

Message Details:

RLC_UM_DATA_IND:

cellId:-1

routingInfo:

rB_Identity:1

integrityResult:

integrityUsed (IntegrityStatus):i_pass

uM_message:

uL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode:10111001101000110000011111000000
rrc_MessageSequenceNumber:2

message: (UL_DCCH_MessageType)

rrcConnectionReleaseComplete:

rrc_TransactionIdentifier:0

errorIndication: (FailureCauseWithProtErr) Omit

laterNonCriticalExtensions: Omit

#### CRLC_Config_REQ

RRC LLA @ 00:00:37.300

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:1

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC UM Channel Release REQ

LLA RLC @ 00:00:37.310

BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 156

Message Details:

#### CRLC UM Channel Release CNF

RLC LLA @ 00:00:37.310

BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 156

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:00:37.320

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:1

#### CRLC_Config_REQ

RRC LLA @ 00:00:37.320

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:2

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC AM Channel Release REQ

LLA RLC @ 00:00:37.320

BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 157

Message Details:

#### CRLC AM Channel Release CNF

RLC LLA @ 00:00:37.320

BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 157

Message Details:

#### CPHY_OUTSYNC_IND

PHY RRC @ 00:00:37.330

BTS unit: 1:1
Channel No: 0 Name: U_DPCH
CFN: 158

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:00:37.330

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:2

#### CRLC_Config_REQ

RRC LLA @ 00:00:37.330

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:3

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC AM Channel Release REQ

LLA RLC @ 00:00:37.340

BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 159

Message Details:

#### CRLC AM Channel Release CNF

RLC LLA @ 00:00:37.340

BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 159

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:00:37.350

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:3

#### CRLC_Config_REQ

RRC LLA @ 00:00:37.350

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:4

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC AM Channel Release REQ

LLA RLC @ 00:00:37.350

BTS unit: 1:1
Channel No: 4 Name: DCCH
CFN: 160

Message Details:

#### CRLC AM Channel Release CNF

RLC LLA @ 00:00:37.350

BTS unit: 1:1
Channel No: 4 Name: DCCH
CFN: 160

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:00:37.360

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:4

#### CRLC_Config_REQ

RRC LLA @ 00:00:37.360

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:1

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode)

dl_UM_RLC_Mode:

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):136

dl_RLCModeInfo: (UL_RLC_Mode)

ul_UM_RLC_Mode:

transmissionRLC_Discard:

timerBasedNoExplicit (NoExplicitDiscard):dt100

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity):1
dLlogicalChannelIdentity (LogicalChannelIdentity):1
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC UM Channel Establish REQ

LLA RLC @ 00:00:37.370

BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 162

Message Details:

Configuration Parameters:

PU Size In Bits:136

#### CRLC UM Channel Establish CNF

RLC LLA @ 00:00:37.370

BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 162

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:00:37.380

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:1

#### CRLC_Config_REQ

RRC LLA @ 00:00:37.380

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:2

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode)

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):128

dl_RLCModeInfo: (UL_RLC_Mode)

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity):2
dLlogicalChannelIdentity (LogicalChannelIdentity):2
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC AM Channel Establish REQ

LLA RLC @ 00:00:37.380

BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 163

Message Details:

Configuration Parameters:

PU Size In Bits:128

Timer Parameters:

Poll (ms):200
Poll Prohibit (ms):0
EPC (ms):0
Discard (ms):0
Poll Periodic (ms):0
Status Prohibit (ms):0
Status Periodic (ms):0
Reset (ms):500
MRW (ms):0

Protocol Parameters:

Max Dat:15
Poll PU:0
Poll SDU:1
Poll Window:99
Max Reset:1
Tx Window Size:32
Rx Window Size:32
Max MRW:0
SDU Discard Mode:No discard

Polling Triggers:

Last PU In Buffer:On
Last PU In Retransmission Buffer:On
Poll Timer:On
Every Poll-PU PU:Off
Every Poll-SDU SDU:On
Poll-Window Percent Of Transmission Buffer:On
Timer Based:Off

Status Triggers:

Missing PU:On
Timer Based:Off
EPC Mechanism:Off

#### CRLC AM Channel Establish CNF

RLC LLA @ 00:00:37.380

BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 163

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:00:37.390

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:2

#### CRLC_Config_REQ

RRC LLA @ 00:00:37.390

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:3

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode)

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):128

dl_RLCModeInfo: (UL_RLC_Mode)

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity):3
dLlogicalChannelIdentity (LogicalChannelIdentity):3
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC AM Channel Establish REQ

LLA RLC @ 00:00:37.400

BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 165

Message Details:

Configuration Parameters:

PU Size In Bits:128

Timer Parameters:

Poll (ms):200
Poll Prohibit (ms):0
EPC (ms):0
Discard (ms):0
Poll Periodic (ms):0
Status Prohibit (ms):0
Status Periodic (ms):0
Reset (ms):500
MRW (ms):0

Protocol Parameters:

Max Dat:15
Poll PU:0
Poll SDU:1
Poll Window:99
Max Reset:1
Tx Window Size:32
Rx Window Size:32
Max MRW:0
SDU Discard Mode:No discard

Polling Triggers:

Last PU In Buffer:On
Last PU In Retransmission Buffer:On
Poll Timer:On
Every Poll-PU PU:Off
Every Poll-SDU SDU:On
Poll-Window Percent Of Transmission Buffer:On
Timer Based:Off

Status Triggers:

Missing PU:On
Timer Based:Off
EPC Mechanism:Off

#### CRLC AM Channel Establish CNF

RLC LLA @ 00:00:37.400

BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 165

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:00:37.410

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:3

#### CRLC_Config_REQ

RRC LLA @ 00:00:37.410

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:4

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode)

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):128

dl_RLCModeInfo: (UL_RLC_Mode)

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity):4
dLlogicalChannelIdentity (LogicalChannelIdentity):4
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC AM Channel Establish REQ

LLA RLC @ 00:00:37.410

BTS unit: 1:1
Channel No: 4 Name: DCCH
CFN: 166

Message Details:

Configuration Parameters:

PU Size In Bits:128

Timer Parameters:

Poll (ms):200
Poll Prohibit (ms):0
EPC (ms):0
Discard (ms):0
Poll Periodic (ms):0
Status Prohibit (ms):0
Status Periodic (ms):0
Reset (ms):500
MRW (ms):0

Protocol Parameters:

Max Dat:15
Poll PU:0
Poll SDU:1
Poll Window:99
Max Reset:1
Tx Window Size:32
Rx Window Size:32
Max MRW:0
SDU Discard Mode:No discard

Polling Triggers:

Last PU In Buffer:On
Last PU In Retransmission Buffer:On
Poll Timer:On
Every Poll-PU PU:Off
Every Poll-SDU SDU:On
Poll-Window Percent Of Transmission Buffer:On
Timer Based:Off

Status Triggers:

Missing PU:On
Timer Based:Off
EPC Mechanism:Off

#### CRLC AM Channel Establish CNF

RLC LLA @ 00:00:37.410

BTS unit: 1:1
Channel No: 4 Name: DCCH
CFN: 166

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:00:37.430

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:4

#### MMI_CmdReq

RRC LLA @ 00:00:42.440

Message Details:

MMI_CmdReq:

cmd (IA5String):Please switch off the UE

#### MMI_CmdCnf

LLA RRC @ 00:00:43.820

Message Details:

MMI_CmdCnf:

result:true
resultString (IA5String): Omit

#### PHY_DATA_IND

PHY MAC @ 00:00:48.260

BTS unit: 1:1
Channel No: 0 Name: U_RACH
CFN: 207

Message Details:

TFI:0
TB set size:168
TB size:168
TB set (raw):

[0]08 44 48 8C D1 00 04 02
[8]00 02 D0 00 00 00 00 00
[16]00 00 00 00 00 00

TB set (decoded):

TB 0:

TCTF:0
MAC SDU (166 bits):

[0]21 11 22 33 44 00 10 08
[8]00 0B 40 00 00 00 00 00
[16]00 00 00 00 00

#### MAC_DATA_IND

MAC RLC @ 00:00:48.260

Category: Configuration
BTS unit: 1:1
Channel No: 0 Name: CCCH
CFN: 207

Message Details:

RLC PDU size (bits):166
RLC PDU (raw):

[0]21 11 22 33 44 00 10 08
[8]00 0B 40 00 00 00 00 00
[16]00 00 00 00 00

#### RLC_TR_DATA_IND: rrcConnectionRequest

RLC LLA @ 00:00:48.290

Channel No: 0 Name: CCCH

Message Details:

UL_CCCH_Message:

integrityCheckInfo: Omitted

message:

rrcConnectionRequest:

initialUE_Identity:

tmsi_and_LAI:

tmsi: 00010001001000100011001101000100

lai:

plmn_Identity:

mcc:

MCC.element: 0

MCC.element: 0

MCC.element: 1

mnc:

MNC.element: 0

MNC.element: 1

lac: 0000000000000001

establishmentCause: detach_EstablishmentCause [enum=13]

protocolErrorIndicator: noError_ProtocolErrorIndicator [enum=0]

measuredResultsOnRACH: Omitted

v3d0NonCriticalExtensions: Omitted

Layer 3 SDU:

[0]21 11 22 33 44 00 10 08
[8]00 0B 40 00 00 00 00 00
[16]00 00 00 00 00

#### RLC_TR_DATA_IND

LLA RRC @ 00:00:48.290

Channel ID: Rb0
Cell ID: 0

Message Details:

RLC_TR_DATA_IND:

cellId:0

routingInfo:

rB_Identity:0

tM_message:

uL_CCCH_Message:

integrityCheckInfo: Omit

message: (UL_CCCH_MessageType)

rrcConnectionRequest:

initialUE_Identity:

tmsi_and_LAI: (TMSI_and_LAI_GSM_MAP)

tmsi (TMSI_GSM_MAP):00010001001000100011001101000100

lai:

plmn_Identity:

mcc:

Digit:0
Digit:0
Digit:1

mnc:

Digit:0
Digit:1

lac:0000000000000001

establishmentCause:detach
protocolErrorIndicator:noError

measuredResultsOnRACH: Omit

v3d0NonCriticalExtensions: Omit

#### RLC_UM_DATA_REQ

RRC LLA @ 00:00:48.290

Channel ID: Rb0
Cell ID: 0

Message Details:

RLC_UM_DATA_REQ:

cellId:0

routingInfo:

rB_Identity:0

uM_message:

dL_CCCH_Message:

integrityCheckInfo: Omit

message: (DL_CCCH_MessageType)

rrcConnectionSetup:

r3:

rrcConnectionSetup_r3: (RRCConnectionSetup_r3_IEs)

initialUE_Identity:

tmsi_and_LAI: (TMSI_and_LAI_GSM_MAP)

tmsi (TMSI_GSM_MAP):00010001001000100011001101000100

lai:

plmn_Identity:

mcc:

Digit:0
Digit:0
Digit:1

mnc:

Digit:0
Digit:1

lac:0000000000000001

rrc_TransactionIdentifier:0
activationTime: Omit

new_U_RNTI: (U_RNTI)

srnc_Identity:000000000001
s_RNTI:00000000000000000001

new_c_RNTI (C_RNTI): Omit
rrc_StateIndicator:cell_DCH
utran_DRX_CycleLengthCoeff (UTRAN_DRX_CycleLengthCoefficient):9

capabilityUpdateRequirement:

ue_RadioCapabilityFDDUpdateRequirement:true
ue_RadioCapabilityTDDUpdateRequirement:false

systemSpecificCapUpdateReqList:

SystemSpecificCapUpdateReq:gsm

srb_InformationSetupList: (SRB_InformationSetupList2)

SRB_InformationSetup:

rb_Identity: Omit

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_UM_RLC_Mode:

transmissionRLC_Discard: Omit

dl_RLC_Mode:

dl_UM_RLC_Mode:

rb_MappingInfo:

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

dch (TransportChannelIdentity):5

logicalChannelIdentity:1

rlc_SizeList:

configured:

mac_LogicalChannelPriority:1

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

dch (TransportChannelIdentity):10

logicalChannelIdentity:1

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

rach:

logicalChannelIdentity:1

rlc_SizeList:

explicitList: (RLC_SizeExplicitList)

RLC_SizeInfo:

rlc_SizeIndex:1

mac_LogicalChannelPriority:1

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

fach:

logicalChannelIdentity:1

SRB_InformationSetup:

rb_Identity: Omit

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

rb_MappingInfo:

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

dch (TransportChannelIdentity):5

logicalChannelIdentity:2

rlc_SizeList:

configured:

mac_LogicalChannelPriority:2

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

dch (TransportChannelIdentity):10

logicalChannelIdentity:2

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

rach:

logicalChannelIdentity:2

rlc_SizeList:

explicitList: (RLC_SizeExplicitList)

RLC_SizeInfo:

rlc_SizeIndex:1

mac_LogicalChannelPriority:2

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

fach:

logicalChannelIdentity:2

SRB_InformationSetup:

rb_Identity: Omit

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

rb_MappingInfo:

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

dch (TransportChannelIdentity):5

logicalChannelIdentity:3

rlc_SizeList:

configured:

mac_LogicalChannelPriority:3

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

dch (TransportChannelIdentity):10

logicalChannelIdentity:3

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

rach:

logicalChannelIdentity:3

rlc_SizeList:

explicitList: (RLC_SizeExplicitList)

RLC_SizeInfo:

rlc_SizeIndex:1

mac_LogicalChannelPriority:3

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

fach:

logicalChannelIdentity:3

SRB_InformationSetup:

rb_Identity: Omit

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

rb_MappingInfo:

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

dch (TransportChannelIdentity):5

logicalChannelIdentity:4

rlc_SizeList:

configured:

mac_LogicalChannelPriority:4

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

dch (TransportChannelIdentity):10

logicalChannelIdentity:4

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

rach:

logicalChannelIdentity:4

rlc_SizeList:

explicitList: (RLC_SizeExplicitList)

RLC_SizeInfo:

rlc_SizeIndex:1

mac_LogicalChannelPriority:4

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

fach:

logicalChannelIdentity:4

ul_CommonTransChInfo:

tfc_Subset: Omit

prach_TFCS: (TFCS) Omit

modeSpecificInfo:

fdd:

ul_TFCS: (TFCS)

normalTFCI_Signalling: (ExplicitTFCS_Configuration)

complete: (TFCS_ReconfAdd)

ctfcSize:

ctfc2Bit:

:

ctfc2:0

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc2:1

powerOffsetInformation:

gainFactorInformation:

signalledGainFactors:

modeSpecificInfo:

fdd:

gainFactorBetaC (GainFactor):11

gainFactorBetaD (GainFactor):15
referenceTFC_ID:0

powerOffsetPp_m: Omit

ul_AddReconfTransChInfoList:

UL_AddReconfTransChInformation:

ul_TransportChannelType (UL_TrCH_Type):dch
transportChannelIdentity:5

transportFormatSet:

dedicatedTransChTFS:

tti:

tti10: (DedicatedDynamicTF_InfoList)

DedicatedDynamicTF_Info:

rlc_Size:

bitMode: (BitModeRLC_SizeInfo)

sizeType2:

part1:2
part2: Omit

numberOfTbSizeList:

NumberOfTransportBlocks:

zero:

NumberOfTransportBlocks:

one:

logicalChannelList:

allSizes:

semistaticTF_Information:

channelCodingType:

convolutional (CodingRate):third

rateMatchingAttribute:192
crc_Size:crc16

dl_CommonTransChInfo:

sccpch_TFCS: (TFCS) Omit

modeSpecificInfo:

fdd:

dl_Parameters:

sameAsUL:

dl_AddReconfTransChInfoList:

DL_AddReconfTransChInformation:

dl_TransportChannelType (DL_TrCH_Type):dch
dl_transportChannelIdentity (TransportChannelIdentity):10

tfs_SignallingMode:

sameAsULTrCH: (UL_TransportChannelIdentity)

ul_TransportChannelType (UL_TrCH_Type):dch
ul_TransportChannelIdentity (TransportChannelIdentity):5

dch_QualityTarget: (QualityTarget)

bler_QualityValue:-20

dummy: (TM_SignallingInfo) Omit

frequencyInfo: Omit

maxAllowedUL_TX_Power: Omit

ul_ChannelRequirement:

ul_DPCH_Info:

ul_DPCH_PowerControlInfo:

fdd:

dpcch_PowerOffset:-40
pc_Preamble:1
sRB_delay:7

powerControlAlgorithm:

algorithm1 (TPC_StepSizeFDD):0

modeSpecificInfo:

fdd:

scramblingCodeType:longSC
scramblingCode (UL_ScramblingCode):0
numberOfDPDCH: Omit
spreadingFactor:sf64
tfci_Existence:true
numberOfFBI_Bits: Omit
puncturingLimit:pl1

dl_CommonInformation:

dl_DPCH_InfoCommon:

cfnHandling:

initialise:

cfntargetsfnframeoffset: Omit

modeSpecificInfo:

fdd:

dl_DPCH_PowerControlInfo:

modeSpecificInfo:

fdd:

dpc_Mode:singleTPC

powerOffsetPilot_pdpdch:0

dl_rate_matching_restriction: Omit

spreadingFactorAndPilot: (SF512_AndPilot)

sfd128 (PilotBits128):pb4

positionFixedOrFlexible:fixed
tfci_Existence:false

modeSpecificInfo:

fdd:

defaultDPCH_OffsetValue (DefaultDPCH_OffsetValueFDD):0

dpch_CompressedModeInfo: Omit

tx_DiversityMode:noDiversity

ssdt_Information: Omit

dl_InformationPerRL_List:

DL_InformationPerRL:

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode:100

pdsch_SHO_DCH_Info: Omit

pdsch_CodeMapping: Omit

dl_DPCH_InfoPerRL:

fdd:

pCPICH_UsageForChannelEst:mayBeUsed
dpch_FrameOffset:0

secondaryCPICH_Info: Omit

dl_ChannelisationCodeList:

DL_ChannelisationCode:

secondaryScramblingCode:1

sf_AndCodeNumber: (SF512_AndCodeNumber)

sf128:0

scramblingCodeChange:noCodeChange

tpc_CombinationIndex:0
ssdt_CellIdentity: Omit
closedLoopTimingAdjMode: Omit

sccpch_InfoforFACH: Omit

laterNonCriticalExtensions: Omit

specialLI:true

#### RLC_UM_DATA_REQ: rrcConnectionSetup

LLA RLC @ 00:00:48.300

Channel No: 1 Name: CCCH

Message Details:

DL_CCCH_Message:

integrityCheckInfo: Omitted

message:

rrcConnectionSetup:

r3:

rrcConnectionSetup_r3:

initialUE_Identity:

tmsi_and_LAI:

tmsi: 00010001001000100011001101000100

lai:

plmn_Identity:

mcc:

MCC.element: 0

MCC.element: 0

MCC.element: 1

mnc:

MNC.element: 0

MNC.element: 1

lac: 0000000000000001

rrc_TransactionIdentifier: 0

activationTime: Omitted

new_U_RNTI:

srnc_Identity: 000000000001

s_RNTI: 00000000000000000001

new_c_RNTI: Omitted

rrc_StateIndicator: cell_DCH_RRC_StateIndicator [enum=0]

utran_DRX_CycleLengthCoeff: 9

capabilityUpdateRequirement:

ue_RadioCapabilityFDDUpdateRequirement: 1

ue_RadioCapabilityTDDUpdateRequirement: 0

systemSpecificCapUpdateReqList:

SystemSpecificCapUpdateReqList.element: gsm_SystemSpecificCapUpdateReq [enum=0]

srb_InformationSetupList:

SRB_InformationSetupList2.element:

rb_Identity: Omitted

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_UM_RLC_Mode:

transmissionRLC_Discard: Omitted

dl_RLC_Mode:

dl_UM_RLC_Mode: NULL

rb_MappingInfo:

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

dch: 5

logicalChannelIdentity: 1

rlc_SizeList:

configured: NULL

mac_LogicalChannelPriority: 1

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

dch: 10

logicalChannelIdentity: 1

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

rach: NULL

logicalChannelIdentity: 1

rlc_SizeList:

explicitList:

RLC_SizeExplicitList.element:

rlc_SizeIndex: 1

mac_LogicalChannelPriority: 1

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

fach: NULL

logicalChannelIdentity: 1

SRB_InformationSetupList2.element:

rb_Identity: Omitted

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard: dat15_MaxDAT [enum=10]

transmissionWindowSize: tw32_TransmissionWindowSize [enum=3]

timerRST: tr500_TimerRST [enum=9]

max_RST: rst1_MaxRST [enum=0]

pollingInfo:

timerPollProhibit: tpp200_TimerPollProhibit [enum=19]

timerPoll: tp200_TimerPoll [enum=19]

poll_PDU: Omitted

poll_SDU: sdu1_Poll_SDU [enum=0]

lastTransmissionPDU_Poll: 1

lastRetransmissionPDU_Poll: 1

pollWindow: pw99_PollWindow [enum=7]

timerPollPeriodic: Omitted

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery: 1

receivingWindowSize: rw32_ReceivingWindowSize [enum=3]

dl_RLC_StatusInfo:

timerStatusProhibit: tsp200_TimerStatusProhibit [enum=19]

timerEPC: Omitted

missingPDU_Indicator: 1

timerStatusPeriodic: Omitted

rb_MappingInfo:

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

dch: 5

logicalChannelIdentity: 2

rlc_SizeList:

configured: NULL

mac_LogicalChannelPriority: 2

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

dch: 10

logicalChannelIdentity: 2

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

rach: NULL

logicalChannelIdentity: 2

rlc_SizeList:

explicitList:

RLC_SizeExplicitList.element:

rlc_SizeIndex: 1

mac_LogicalChannelPriority: 2

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

fach: NULL

logicalChannelIdentity: 2

SRB_InformationSetupList2.element:

rb_Identity: Omitted

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard: dat15_MaxDAT [enum=10]

transmissionWindowSize: tw32_TransmissionWindowSize [enum=3]

timerRST: tr500_TimerRST [enum=9]

max_RST: rst1_MaxRST [enum=0]

pollingInfo:

timerPollProhibit: tpp200_TimerPollProhibit [enum=19]

timerPoll: tp200_TimerPoll [enum=19]

poll_PDU: Omitted

poll_SDU: sdu1_Poll_SDU [enum=0]

lastTransmissionPDU_Poll: 1

lastRetransmissionPDU_Poll: 1

pollWindow: pw99_PollWindow [enum=7]

timerPollPeriodic: Omitted

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery: 1

receivingWindowSize: rw32_ReceivingWindowSize [enum=3]

dl_RLC_StatusInfo:

timerStatusProhibit: tsp200_TimerStatusProhibit [enum=19]

timerEPC: Omitted

missingPDU_Indicator: 1

timerStatusPeriodic: Omitted

rb_MappingInfo:

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

dch: 5

logicalChannelIdentity: 3

rlc_SizeList:

configured: NULL

mac_LogicalChannelPriority: 3

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

dch: 10

logicalChannelIdentity: 3

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

rach: NULL

logicalChannelIdentity: 3

rlc_SizeList:

explicitList:

RLC_SizeExplicitList.element:

rlc_SizeIndex: 1

mac_LogicalChannelPriority: 3

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

fach: NULL

logicalChannelIdentity: 3

SRB_InformationSetupList2.element:

rb_Identity: Omitted

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard: dat15_MaxDAT [enum=10]

transmissionWindowSize: tw32_TransmissionWindowSize [enum=3]

timerRST: tr500_TimerRST [enum=9]

max_RST: rst1_MaxRST [enum=0]

pollingInfo:

timerPollProhibit: tpp200_TimerPollProhibit [enum=19]

timerPoll: tp200_TimerPoll [enum=19]

poll_PDU: Omitted

poll_SDU: sdu1_Poll_SDU [enum=0]

lastTransmissionPDU_Poll: 1

lastRetransmissionPDU_Poll: 1

pollWindow: pw99_PollWindow [enum=7]

timerPollPeriodic: Omitted

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery: 1

receivingWindowSize: rw32_ReceivingWindowSize [enum=3]

dl_RLC_StatusInfo:

timerStatusProhibit: tsp200_TimerStatusProhibit [enum=19]

timerEPC: Omitted

missingPDU_Indicator: 1

timerStatusPeriodic: Omitted

rb_MappingInfo:

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

dch: 5

logicalChannelIdentity: 4

rlc_SizeList:

configured: NULL

mac_LogicalChannelPriority: 4

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

dch: 10

logicalChannelIdentity: 4

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

rach: NULL

logicalChannelIdentity: 4

rlc_SizeList:

explicitList:

RLC_SizeExplicitList.element:

rlc_SizeIndex: 1

mac_LogicalChannelPriority: 4

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

fach: NULL

logicalChannelIdentity: 4

ul_CommonTransChInfo:

tfc_Subset: Omitted

prach_TFCS: Omitted

modeSpecificInfo:

fdd:

ul_TFCS:

normalTFCI_Signalling:

complete:

ctfcSize:

ctfc2Bit:

ctfc2Bit.noName:

ctfc2: 0

powerOffsetInformation:

gainFactorInformation:

computedGainFactors: 0

powerOffsetPp_m: Omitted

ctfc2Bit.noName:

ctfc2: 1

powerOffsetInformation:

gainFactorInformation:

signalledGainFactors:

modeSpecificInfo:

fdd:

gainFactorBetaC: 11

gainFactorBetaD: 15

referenceTFC_ID: 0

powerOffsetPp_m: Omitted

ul_AddReconfTransChInfoList:

UL_AddReconfTransChInfoList.element:

ul_TransportChannelType: dch_UL_TrCH_Type [enum=0]

transportChannelIdentity: 5

transportFormatSet:

dedicatedTransChTFS:

tti:

tti10:

DedicatedDynamicTF_InfoList.element:

rlc_Size:

bitMode:

sizeType2:

part1: 2

part2: Omitted

numberOfTbSizeList:

numberOfTbSizeList.element:

zero: NULL

numberOfTbSizeList.element:

one: NULL

logicalChannelList:

allSizes: NULL

semistaticTF_Information:

channelCodingType:

convolutional: third_CodingRate [enum=1]

rateMatchingAttribute: 192

crc_Size: crc16_CRC_Size [enum=3]

dl_CommonTransChInfo:

sccpch_TFCS: Omitted

modeSpecificInfo:

fdd:

dl_Parameters:

sameAsUL: NULL

dl_AddReconfTransChInfoList:

DL_AddReconfTransChInfoList.element:

dl_TransportChannelType: dch_DL_TrCH_Type [enum=0]

dl_transportChannelIdentity: 10

tfs_SignallingMode:

sameAsULTrCH:

ul_TransportChannelType: dch_UL_TrCH_Type [enum=0]

ul_TransportChannelIdentity: 5

dch_QualityTarget:

bler_QualityValue: -20

dummy: Omitted

frequencyInfo: Omitted

maxAllowedUL_TX_Power: Omitted

ul_ChannelRequirement:

ul_DPCH_Info:

ul_DPCH_PowerControlInfo:

fdd:

dpcch_PowerOffset: -40

pc_Preamble: 1

sRB_delay: 7

powerControlAlgorithm:

algorithm1: 0

modeSpecificInfo:

fdd:

scramblingCodeType: longSC_ScramblingCodeType [enum=1]

scramblingCode: 0

numberOfDPDCH: Default

spreadingFactor: sf64_SpreadingFactor [enum=4]

tfci_Existence: 1

numberOfFBI_Bits: Omitted

puncturingLimit: pl1_PuncturingLimit [enum=15]

dl_CommonInformation:

dl_DPCH_InfoCommon:

cfnHandling:

initialise:

cfntargetsfnframeoffset: Omitted

modeSpecificInfo:

fdd:

dl_DPCH_PowerControlInfo:

modeSpecificInfo:

fdd:

dpc_Mode: singleTPC_DPC_Mode [enum=0]

powerOffsetPilot_pdpdch: 0

dl_rate_matching_restriction: Omitted

spreadingFactorAndPilot:

sfd128: pb4_PilotBits128 [enum=0]

positionFixedOrFlexible: fixed_PositionFixedOrFlexible [enum=0]

tfci_Existence: 0

modeSpecificInfo:

fdd:

defaultDPCH_OffsetValue: 0

dpch_CompressedModeInfo: Omitted

tx_DiversityMode: noDiversity_TX_DiversityMode [enum=0]

ssdt_Information: Omitted

dl_InformationPerRL_List:

DL_InformationPerRL_List.element:

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode: 100

pdsch_SHO_DCH_Info: Omitted

pdsch_CodeMapping: Omitted

dl_DPCH_InfoPerRL:

fdd:

pCPICH_UsageForChannelEst: mayBeUsed_PCPICH_UsageForChannelEst [enum=0]

dpch_FrameOffset: 0

secondaryCPICH_Info: Omitted

dl_ChannelisationCodeList:

DL_ChannelisationCodeList.element:

secondaryScramblingCode: 1

sf_AndCodeNumber:

sf128: 0

scramblingCodeChange: noCodeChange_ScramblingCodeChange [enum=1]

tpc_CombinationIndex: 0

ssdt_CellIdentity: Omitted

closedLoopTimingAdjMode: Omitted

sccpch_InfoforFACH: Omitted

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]30 E7 22 24 46 68 80 02
[8]01 00 01 00 04 00 00 4D
[16]82 69 3A 10 10 89 0D 42
[24]00 02 81 9E 8E 46 C9 A6
[32]7C 9C 4E 74 20 A5 12 3A
[40]8C 00 15 13 3D 1C 8D 93
[48]4C F9 38 9C E8 42 52 24
[56]B5 28 00 4A 46 7A 39 1B
[64]26 99 F2 71 39 D0 86 B4
[72]49 EA 70 00 D4 C8 00 06
[80]25 2B F0 02 00 08 82 23
[88]BF 66 08 98 95 A5 47 82
[96]00 00 01 3F 90 0A 14 00
[104]02 06 40 00 0C 28 08

#### MAC_DATA_REQ

RLC MAC @ 00:00:48.330

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: CCCH
CFN: 234

Message Details:

RLC PDU size (bits):160
RLC PDU (raw):

[0]0D F8 30 E7 22 24 46 68
[8]80 02 01 00 01 00 04 00
[16]00 4D 82 69

RLC PDU (decoded):

Sequence number:6
Length indicator 0 (octets):124 (the first data octet in this RLC PDU is the first octet of a RLC SDU)
Segment associated with length indicator 0 (0 octets):

Last segment, not associated with any length indicators (18 octets):

[0]30 E7 22 24 46 68 80 02
[8]01 00 01 00 04 00 00 4D
[16]82 69

#### MAC_DATA_REQ

RLC MAC @ 00:00:48.330

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: CCCH
CFN: 234

Message Details:

RLC PDU size (bits):160
RLC PDU (raw):

[0]0E 3A 10 10 89 0D 42 00
[8]02 81 9E 8E 46 C9 A6 7C
[16]9C 4E 74 20

RLC PDU (decoded):

Sequence number:7
Last segment, not associated with any length indicators (19 octets):

[0]3A 10 10 89 0D 42 00 02
[8]81 9E 8E 46 C9 A6 7C 9C
[16]4E 74 20

#### MAC_DATA_REQ

RLC MAC @ 00:00:48.330

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: CCCH
CFN: 234

Message Details:

RLC PDU size (bits):160
RLC PDU (raw):

[0]10 A5 12 3A 8C 00 15 13
[8]3D 1C 8D 93 4C F9 38 9C
[16]E8 42 52 24

RLC PDU (decoded):

Sequence number:8
Last segment, not associated with any length indicators (19 octets):

[0]A5 12 3A 8C 00 15 13 3D
[8]1C 8D 93 4C F9 38 9C E8
[16]42 52 24

#### MAC_DATA_REQ

RLC MAC @ 00:00:48.330

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: CCCH
CFN: 234

Message Details:

RLC PDU size (bits):160
RLC PDU (raw):

[0]12 B5 28 00 4A 46 7A 39
[8]1B 26 99 F2 71 39 D0 86
[16]B4 49 EA 70

RLC PDU (decoded):

Sequence number:9
Last segment, not associated with any length indicators (19 octets):

[0]B5 28 00 4A 46 7A 39 1B
[8]26 99 F2 71 39 D0 86 B4
[16]49 EA 70

#### MAC_DATA_REQ

RLC MAC @ 00:00:48.330

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: CCCH
CFN: 234

Message Details:

RLC PDU size (bits):160
RLC PDU (raw):

[0]14 00 D4 C8 00 06 25 2B
[8]F0 02 00 08 82 23 BF 66
[16]08 98 95 A5

RLC PDU (decoded):

Sequence number:10
Last segment, not associated with any length indicators (19 octets):

[0]00 D4 C8 00 06 25 2B F0
[8]02 00 08 82 23 BF 66 08
[16]98 95 A5

#### MAC_DATA_REQ

RLC MAC @ 00:00:48.330

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: CCCH
CFN: 234

Message Details:

RLC PDU size (bits):160
RLC PDU (raw):

[0]17 23 FE 47 82 00 00 01
[8]3F 90 0A 14 00 02 06 40
[16]00 0C 28 08

RLC PDU (decoded):

Sequence number:11
Length indicator 0 (octets):17
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (17 octets):

[0]47 82 00 00 01 3F 90 0A
[8]14 00 02 06 40 00 0C 28
[16]08
Padding associated with length indicator 1 (0 octets):

#### PHY_DATA_REQ

MAC PHY @ 00:00:48.330

BTS unit: 1:1
Channel No: 0 Name: FACH
CFN: 234

Message Details:

TFI:2
TB set size:336
TB size:168
TB set (raw, each TB word aligned):

[0]40 0D F8 30 E7 22 24 46
[8]68 80 02 01 00 01 00 04
[16]00 00 4D 82 69 00 40 0E
[24]3A 10 10 89 0D 42 00 02
[32]81 9E 8E 46 C9 A6 7C 9C
[40]4E 74 20 00

TB set (decoded):

TB 0:

TCTF:64
MAC SDU (160 bits):

[0]0D F8 30 E7 22 24 46 68
[8]80 02 01 00 01 00 04 00
[16]00 4D 82 69

TB 1:

TCTF:64
MAC SDU (160 bits):

[0]0E 3A 10 10 89 0D 42 00
[8]02 81 9E 8E 46 C9 A6 7C
[16]9C 4E 74 20

#### PHY_DATA_REQ

MAC PHY @ 00:00:48.340

BTS unit: 1:1
Channel No: 0 Name: FACH
CFN: 235

Message Details:

TFI:2
TB set size:336
TB size:168
TB set (raw, each TB word aligned):

[0]40 10 A5 12 3A 8C 00 15
[8]13 3D 1C 8D 93 4C F9 38
[16]9C E8 42 52 24 00 40 12
[24]B5 28 00 4A 46 7A 39 1B
[32]26 99 F2 71 39 D0 86 B4
[40]49 EA 70 00

TB set (decoded):

TB 0:

TCTF:64
MAC SDU (160 bits):

[0]10 A5 12 3A 8C 00 15 13
[8]3D 1C 8D 93 4C F9 38 9C
[16]E8 42 52 24

TB 1:

TCTF:64
MAC SDU (160 bits):

[0]12 B5 28 00 4A 46 7A 39
[8]1B 26 99 F2 71 39 D0 86
[16]B4 49 EA 70

#### PHY_DATA_REQ

MAC PHY @ 00:00:48.350

BTS unit: 1:1
Channel No: 0 Name: FACH
CFN: 236

Message Details:

TFI:2
TB set size:336
TB size:168
TB set (raw, each TB word aligned):

[0]40 14 00 D4 C8 00 06 25
[8]2B F0 02 00 08 82 23 BF
[16]66 08 98 95 A5 00 40 17
[24]23 FE 47 82 00 00 01 3F
[32]90 0A 14 00 02 06 40 00
[40]0C 28 08 00

TB set (decoded):

TB 0:

TCTF:64
MAC SDU (160 bits):

[0]14 00 D4 C8 00 06 25 2B
[8]F0 02 00 08 82 23 BF 66
[16]08 98 95 A5

TB 1:

TCTF:64
MAC SDU (160 bits):

[0]17 23 FE 47 82 00 00 01
[8]3F 90 0A 14 00 02 06 40
[16]00 0C 28 08

#### CPHY_SYNC_IND

PHY RRC @ 00:00:48.570

BTS unit: 1:1
Channel No: 0 Name: U_DPCH
CFN: 2

Message Details:

#### PHY_DATA_IND

PHY MAC @ 00:00:48.730

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 254

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 00 04 B0 C0 00 08 00
[8]00 51 1B 8D D0 6A 4C 66
[16]88 A2 C0 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 00 4B 0C 00 00 80 00
[8]05 11 B8 DD 06 A4 C6 68
[16]8A 2C

#### MAC_DATA_IND

MAC RLC @ 00:00:48.730

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 254

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 00 4B 0C 00 00 80 00
[8]05 11 B8 DD 06 A4 C6 68
[16]8A 2C

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:0
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]4B 0C 00 00 80 00 05 11
[8]B8 DD 06 A4 C6 68 8A 2C

#### PHY_DATA_IND

PHY MAC @ 00:00:48.740

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 255

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 00 88 30 34 80 01 80
[8]01 18 FC FC 0C C0 D5 C6
[16]28 48 C0 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 08 83 03 48 00 18 00
[8]11 8F CF C0 CC 0D 5C 62
[16]84 8C

#### MAC_DATA_IND

MAC RLC @ 00:00:48.740

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 255

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 08 83 03 48 00 18 00
[8]11 8F CF C0 CC 0D 5C 62
[16]84 8C

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:1
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]83 03 48 00 18 00 11 8F
[8]CF C0 CC 0D 5C 62 84 8C

#### PHY_DATA_IND

PHY MAC @ 00:00:48.750

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 0

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 01 50 BF E0 28 99 01
[8]00 05 55 55 55 55 55 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 15 0B FE 02 89 90 10
[8]00 55 55 55 55 55 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:00:48.750

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 0

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 15 0B FE 02 89 90 10
[8]00 55 55 55 55 55 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:2
Polling bit:1 (request a status report)
Length indicator 0 (octets):5
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (5 octets):

[0]02 89 90 10 00
Padding associated with length indicator 1 (9 octets):

[0]55 55 55 55 55 55 55 55
[8]55

#### MAC_DATA_REQ

RLC MAC @ 00:00:48.760

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 21

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:3

#### PHY_DATA_REQ

MAC PHY @ 00:00:48.760

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 21

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]10 20 03 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:00:48.760

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 1

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 00 01 58 0D 10 07 04
[8]02 85 8C 02 FA 09 1A 2B
[16]3C 0C 80 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 00 15 80 D1 00 70 40
[8]28 58 C0 2F A0 91 A2 B3
[16]C0 C8

#### MAC_DATA_IND

MAC RLC @ 00:00:48.760

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 1

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 00 15 80 D1 00 70 40
[8]28 58 C0 2F A0 91 A2 B3
[16]C0 C8

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:0
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]15 80 D1 00 70 40 28 58
[8]C0 2F A0 91 A2 B3 C0 C8

#### PHY_DATA_IND

PHY MAC @ 00:00:48.770

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 2

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 00 D0 FF E1 D5 89 1A
[8]20 00 04 05 55 55 55 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 0D 0F FE 1D 58 91 A2
[8]00 00 40 55 55 55 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:00:48.770

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 2

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 0D 0F FE 1D 58 91 A2
[8]00 00 40 55 55 55 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:1
Polling bit:1 (request a status report)
Length indicator 0 (octets):7
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (7 octets):

[0]1D 58 91 A2 00 00 40
Padding associated with length indicator 1 (7 octets):

[0]55 55 55 55 55 55 55

#### RLC_AM_DATA_IND: rrcConnectionSetupComplete

RLC LLA @ 00:00:48.770

Channel No: 2 Name: DCCH

Message Details:

UL_DCCH_Message:

integrityCheckInfo: Omitted

message:

rrcConnectionSetupComplete:

rrc_TransactionIdentifier: 0

startList:

STARTList.element:

cn_DomainIdentity: ps_domain_CN_DomainIdentity [enum=1]

start_Value: 00000000000000000010

STARTList.element:

cn_DomainIdentity: cs_domain_CN_DomainIdentity [enum=0]

start_Value: 00000000000000000010

ue_RadioAccessCapability:

accessStratumReleaseIndicator: r99_AccessStratumReleaseIndicator [enum=0]

pdcp_Capability:

losslessSRNS_RelocationSupport: 0

supportForRfc2507:

notSupported: NULL

rlc_Capability:

totalRLC_AM_BufferSize: kb50_TotalRLC_AM_BufferSize [enum=2]

maximumRLC_WindowSize: mws2047_MaximumRLC_WindowSize [enum=0]

maximumAM_EntityNumber: am6_MaximumAM_EntityNumberRLC_Cap [enum=3]

transportChannelCapability:

dl_TransChCapability:

maxNoBitsReceived: b8960_MaxNoBits [enum=7]

maxConvCodeBitsReceived: b1280_MaxNoBits [enum=1]

turboDecodingSupport:

supported: b8960_MaxNoBits [enum=7]

maxSimultaneousTransChs: e8_MaxSimultaneousTransChsDL [enum=1]

maxSimultaneousCCTrCH_Count: 1

maxReceivedTransportBlocks: tb32_MaxTransportBlocksDL [enum=3]

maxNumberOfTFC: tfc128_MaxNumberOfTFC_DL [enum=5]

maxNumberOfTF: tf64_MaxNumberOfTF [enum=1]

ul_TransChCapability:

maxNoBitsTransmitted: b3840_MaxNoBits [enum=3]

maxConvCodeBitsTransmitted: b1280_MaxNoBits [enum=1]

turboEncodingSupport:

supported: b3840_MaxNoBits [enum=3]

maxSimultaneousTransChs: e8_MaxSimultaneousTransChsUL [enum=2]

modeSpecificInfo:

fdd: NULL

maxTransmittedBlocks: tb32_MaxTransportBlocksUL [enum=4]

maxNumberOfTFC: tfc64_MaxNumberOfTFC_UL [enum=5]

maxNumberOfTF: tf32_MaxNumberOfTF [enum=0]

rf_Capability:

fddRF_Capability:

ue_PowerClass: 4

txRxFrequencySeparation: mhz190_TxRxFrequencySeparation [enum=0]

tddRF_Capability: Omitted

physicalChannelCapability:

fddPhysChCapability:

downlinkPhysChCapability:

maxNoDPCH_PDSCH_Codes: 1

maxNoPhysChBitsReceived: b9600_MaxNoPhysChBitsReceived [enum=6]

supportForSF_512: 0

supportOfPDSCH: 0

simultaneousSCCPCH_DPCH_Reception:

notSupported: NULL

uplinkPhysChCapability:

maxNoDPDCH_BitsTransmitted: b4800_MaxNoDPDCH_BitsTransmitted [enum=3]

supportOfPCPCH: 0

tddPhysChCapability: Omitted

ue_MultiModeRAT_Capability:

multiRAT_CapabilityList:

supportOfGSM: 1

supportOfMulticarrier: 0

multiModeCapability: fdd_MultiModeCapability [enum=1]

securityCapability:

cipheringAlgorithmCap: 0000000000000011

integrityProtectionAlgorithmCap: 0000000000000010

ue_positioning_Capability:

standaloneLocMethodsSupported: 0

ue_BasedOTDOA_Supported: 0

networkAssistedGPS_Supported: noNetworkAssistedGPS_NetworkAssistedGPS_Supported [enum=3]

supportForUE_GPS_TimingOfCellFrames: 0

supportForIPDL: 0

measurementCapability:

downlinkCompressedMode:

fdd_Measurements: 1

tdd_Measurements: Omitted

gsm_Measurements:

gsm900: 1

dcs1800: 1

gsm1900: 1

multiCarrierMeasurements: 0

uplinkCompressedMode:

fdd_Measurements: 1

tdd_Measurements: Omitted

gsm_Measurements:

gsm900: 1

dcs1800: 1

gsm1900: 1

multiCarrierMeasurements: 0

ue_RATSpecificCapability:

InterRAT_UE_RadioAccessCapabilityList.element:

gsm:

gsm_Classmark2: 33035718A1

gsm_Classmark3: 60144C8080

v370NonCriticalExtensions: Omitted

Layer 3 SDU:

[0]4B 0C 00 00 80 00 05 11
[8]B8 DD 06 A4 C6 68 8A 2C
[16]83 03 48 00 18 00 11 8F
[24]CF C0 CC 0D 5C 62 84 8C
[32]02 89 90 10 00

#### RLC_AM_DATA_IND

LLA RRC @ 00:00:48.770

Channel ID: Rb2
Cell ID: -1

Message Details:

RLC_AM_DATA_IND:

cellId:-1

routingInfo:

rB_Identity:2

integrityResult:

integrityUsed (IntegrityStatus):i_pass

aM_message:

uL_DCCH_Message:

integrityCheckInfo: Omit

message: (UL_DCCH_MessageType)

rrcConnectionSetupComplete:

rrc_TransactionIdentifier:0

startList:

STARTSingle:

cn_DomainIdentity:ps_domain
start_Value:00000000000000000010

STARTSingle:

cn_DomainIdentity:cs_domain
start_Value:00000000000000000010

ue_RadioAccessCapability:

accessStratumReleaseIndicator:r99

pdcp_Capability:

losslessSRNS_RelocationSupport:false

supportForRfc2507:

notSupported:

rlc_Capability:

totalRLC_AM_BufferSize:kb50
maximumRLC_WindowSize:mws2047
maximumAM_EntityNumber (MaximumAM_EntityNumberRLC_Cap):am6

transportChannelCapability:

dl_TransChCapability:

maxNoBitsReceived (MaxNoBits):b8960
maxConvCodeBitsReceived (MaxNoBits):b1280

turboDecodingSupport: (TurboSupport)

supported (MaxNoBits):b8960

maxSimultaneousTransChs (MaxSimultaneousTransChsDL):e8
maxSimultaneousCCTrCH_Count:1
maxReceivedTransportBlocks (MaxTransportBlocksDL):tb32
maxNumberOfTFC (MaxNumberOfTFC_DL):tfc128
maxNumberOfTF:tf64

ul_TransChCapability:

maxNoBitsTransmitted (MaxNoBits):b3840
maxConvCodeBitsTransmitted (MaxNoBits):b1280

turboEncodingSupport: (TurboSupport)

supported (MaxNoBits):b3840

maxSimultaneousTransChs (MaxSimultaneousTransChsUL):e8

modeSpecificInfo:

fdd:

maxTransmittedBlocks (MaxTransportBlocksUL):tb32
maxNumberOfTFC (MaxNumberOfTFC_UL):tfc64
maxNumberOfTF:tf32

rf_Capability:

fddRF_Capability:

ue_PowerClass:4
txRxFrequencySeparation:mhz190

tddRF_Capability: Omit

physicalChannelCapability:

fddPhysChCapability:

downlinkPhysChCapability: (DL_PhysChCapabilityFDD)

maxNoDPCH_PDSCH_Codes:1
maxNoPhysChBitsReceived:b9600
supportForSF_512:false
supportOfPDSCH:false

simultaneousSCCPCH_DPCH_Reception:

notSupported:

uplinkPhysChCapability: (UL_PhysChCapabilityFDD)

maxNoDPDCH_BitsTransmitted:b4800
supportOfPCPCH:false

tddPhysChCapability: Omit

ue_MultiModeRAT_Capability:

multiRAT_CapabilityList: (MultiRAT_Capability)

supportOfGSM:true
supportOfMulticarrier:false

multiModeCapability:fdd

securityCapability:

cipheringAlgorithmCap:0000000000000011
integrityProtectionAlgorithmCap:0000000000000010

ue_positioning_Capability:

standaloneLocMethodsSupported:false
ue_BasedOTDOA_Supported:false
networkAssistedGPS_Supported:noNetworkAssistedGPS
supportForUE_GPS_TimingOfCellFrames:false
supportForIPDL:false

measurementCapability:

downlinkCompressedMode: (CompressedModeMeasCapability)

fdd_Measurements:true
tdd_Measurements: Omit

gsm_Measurements:

gsm900:true
dcs1800:true
gsm1900:true

multiCarrierMeasurements:false

uplinkCompressedMode: (CompressedModeMeasCapability)

fdd_Measurements:true
tdd_Measurements: Omit

gsm_Measurements:

gsm900:true
dcs1800:true
gsm1900:true

multiCarrierMeasurements:false

ue_RATSpecificCapability: (InterRAT_UE_RadioAccessCapabilityList)

InterRAT_UE_RadioAccessCapability:

gsm:

gsm_Classmark2:

[0]33 03 57 18 A1
gsm_Classmark3:

[0]60 14 4C 80 80

v370NonCriticalExtensions: Omit

#### RLC_AM_DATA_IND: initialDirectTransfer

RLC RRC @ 00:00:48.780

Channel No: 3 Name: DCCH

Message Details:

UL_DCCH_Message:

integrityCheckInfo: Omitted

message:

initialDirectTransfer:

cn_DomainIdentity: ps_domain_CN_DomainIdentity [enum=1]

intraDomainNasNodeSelector:

version:

release99:

cn_Type:

gsm_Map_IDNNS:

routingbasis:

localPTMSI:

routingparameter: 0011010001

enteredparameter: 0

nas_Message: 08050B1805F4123456781903AB1234

measuredResultsOnRACH: Omitted

v3a0NonCriticalExtensions:

initialDirectTransfer_v3a0ext:

start_Value: 00000000000000000010

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]15 80 D1 00 70 40 28 58
[8]C0 2F A0 91 A2 B3 C0 C8
[16]1D 58 91 A2 00 00 40

#### RRC_DATA_IND: gmm:detachRequest

RRC NAS @ 00:00:48.780

Cell ID: -1

Message Details:

DETACHREQUESTMO:

skipIndicator: 0000

gMMProtocolDiscriminator: 1000

msgType: 00000101

spare4: 0000

detachType:

powOff: 1

type: 011

ptmsi:

iei: 00011000

iel: 05

iDigit1: 1111

oddEvenInd: 0

typeOfId: 100

otherDigits: 12345678

ptmsiSignature:

iei: 00011001

iel: 03

value: AB1234

#### MAC_DATA_REQ

RLC MAC @ 00:00:48.780

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 23

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 20 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:2

#### PHY_DATA_REQ

MAC PHY @ 00:00:48.780

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 23

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 02 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 20 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:00:48.960

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 21

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 01 50 BF E0 28 99 01
[8]00 05 55 55 55 55 55 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 15 0B FE 02 89 90 10
[8]00 55 55 55 55 55 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:00:48.960

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 21

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 15 0B FE 02 89 90 10
[8]00 55 55 55 55 55 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:2
Polling bit:1 (request a status report)
Length indicator 0 (octets):5
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (5 octets):

[0]02 89 90 10 00
Padding associated with length indicator 1 (9 octets):

[0]55 55 55 55 55 55 55 55
[8]55

#### MAC_DATA_REQ

RLC MAC @ 00:00:48.970

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 42

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:3

#### PHY_DATA_REQ

MAC PHY @ 00:00:48.970

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 42

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]10 20 03 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:00:48.980

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 23

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 00 D0 FF E1 D5 89 1A
[8]20 00 04 05 55 55 55 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 0D 0F FE 1D 58 91 A2
[8]00 00 40 55 55 55 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:00:48.980

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 23

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 0D 0F FE 1D 58 91 A2
[8]00 00 40 55 55 55 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:1
Polling bit:1 (request a status report)
Length indicator 0 (octets):7
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (7 octets):

[0]1D 58 91 A2 00 00 40
Padding associated with length indicator 1 (7 octets):

[0]55 55 55 55 55 55 55

#### MAC_DATA_REQ

RLC MAC @ 00:00:48.990

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 44

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 20 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:2

#### PHY_DATA_REQ

MAC PHY @ 00:00:48.990

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 44

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 02 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 20 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### RLC_UM_DATA_REQ

RRC LLA @ 00:00:49.820

Channel ID: Rb1
Cell ID: -1

Message Details:

RLC_UM_DATA_REQ:

cellId:-1

routingInfo:

rB_Identity:1

uM_message:

dL_DCCH_Message:

integrityCheckInfo: Omit

message: (DL_DCCH_MessageType)

rrcConnectionRelease:

r3:

rrcConnectionRelease_r3: (RRCConnectionRelease_r3_IEs)

rrc_TransactionIdentifier:0
n_308:1
releaseCause:normalEvent

rplmn_information: Omit

laterNonCriticalExtensions: Omit

specialLI:false

#### RLC_UM_DATA_REQ: rrcConnectionRelease

LLA RLC @ 00:00:49.820

Channel No: 1 Name: DCCH

Message Details:

DL_DCCH_Message:

integrityCheckInfo: Omitted

message:

rrcConnectionRelease:

r3:

rrcConnectionRelease_r3:

rrc_TransactionIdentifier: 0

n_308: 1

releaseCause: normalEvent_ReleaseCause [enum=0]

rplmn_information: Omitted

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]3C 80 00

#### MAC_DATA_REQ

RLC MAC @ 00:00:49.820

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 127

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]01 07 FE 3C 80 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

Sequence number:0
Length indicator 0 (octets):3
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (3 octets):

[0]3C 80 00
Padding associated with length indicator 1 (12 octets):

[0]00 00 00 00 00 00 00 00
[8]00 00 00 00

#### PHY_DATA_REQ

MAC PHY @ 00:00:49.820

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 127

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]00 10 7F E3 C8 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:0
MAC SDU (144 bits):

[0]01 07 FE 3C 80 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:00:50.060

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 131

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]00 10 5F E4 40 05 55 55
[8]55 55 55 55 55 55 55 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:0
MAC SDU (144 bits):

[0]01 05 FE 44 00 55 55 55
[8]55 55 55 55 55 55 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:00:50.060

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 131

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]01 05 FE 44 00 55 55 55
[8]55 55 55 55 55 55 55 55
[16]55 55

RLC PDU (decoded):

Sequence number:0
Length indicator 0 (octets):2
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (2 octets):

[0]44 00
Padding associated with length indicator 1 (13 octets):

[0]55 55 55 55 55 55 55 55
[8]55 55 55 55 55

#### RLC_UM_DATA_IND: rrcConnectionReleaseComplete

RLC LLA @ 00:00:50.080

Channel No: 1 Name: DCCH

Message Details:

UL_DCCH_Message:

integrityCheckInfo: Omitted

message:

rrcConnectionReleaseComplete:

rrc_TransactionIdentifier: 0

errorIndication: Omitted

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]44 00

#### RLC_UM_DATA_IND

LLA RRC @ 00:00:50.080

Channel ID: Rb1
Cell ID: -1

Message Details:

RLC_UM_DATA_IND:

cellId:-1

routingInfo:

rB_Identity:1

integrityResult:

integrityUsed (IntegrityStatus):i_pass

uM_message:

uL_DCCH_Message:

integrityCheckInfo: Omit

message: (UL_DCCH_MessageType)

rrcConnectionReleaseComplete:

rrc_TransactionIdentifier:0

errorIndication: (FailureCauseWithProtErr) Omit

laterNonCriticalExtensions: Omit

#### PHY_DATA_IND

PHY MAC @ 00:00:50.220

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 147

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]00 30 5F E4 40 05 55 55
[8]55 55 55 55 55 55 55 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:0
MAC SDU (144 bits):

[0]03 05 FE 44 00 55 55 55
[8]55 55 55 55 55 55 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:00:50.220

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 147

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]03 05 FE 44 00 55 55 55
[8]55 55 55 55 55 55 55 55
[16]55 55

RLC PDU (decoded):

Sequence number:1
Length indicator 0 (octets):2
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (2 octets):

[0]44 00
Padding associated with length indicator 1 (13 octets):

[0]55 55 55 55 55 55 55 55
[8]55 55 55 55 55

#### RLC_UM_DATA_IND: rrcConnectionReleaseComplete

RLC LLA @ 00:00:50.250

Channel No: 1 Name: DCCH

Message Details:

UL_DCCH_Message:

integrityCheckInfo: Omitted

message:

rrcConnectionReleaseComplete:

rrc_TransactionIdentifier: 0

errorIndication: Omitted

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]44 00

#### RLC_UM_DATA_IND

LLA RRC @ 00:00:50.250

Channel ID: Rb1
Cell ID: -1

Message Details:

RLC_UM_DATA_IND:

cellId:-1

routingInfo:

rB_Identity:1

integrityResult:

integrityUsed (IntegrityStatus):i_pass

uM_message:

uL_DCCH_Message:

integrityCheckInfo: Omit

message: (UL_DCCH_MessageType)

rrcConnectionReleaseComplete:

rrc_TransactionIdentifier:0

errorIndication: (FailureCauseWithProtErr) Omit

laterNonCriticalExtensions: Omit

#### CRLC_Config_REQ

RRC LLA @ 00:00:50.250

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:1

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC UM Channel Release REQ

LLA RLC @ 00:00:50.260

BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 171

Message Details:

#### CRLC UM Channel Release CNF

RLC LLA @ 00:00:50.260

BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 171

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:00:50.270

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:1

#### CRLC_Config_REQ

RRC LLA @ 00:00:50.270

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:2

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC AM Channel Release REQ

LLA RLC @ 00:00:50.270

BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 172

Message Details:

#### CRLC AM Channel Release CNF

RLC LLA @ 00:00:50.270

BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 172

Message Details:

#### CPHY_OUTSYNC_IND

PHY RRC @ 00:00:50.280

BTS unit: 1:1
Channel No: 0 Name: U_DPCH
CFN: 173

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:00:50.290

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:2

#### CRLC_Config_REQ

RRC LLA @ 00:00:50.290

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:3

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC AM Channel Release REQ

LLA RLC @ 00:00:50.290

BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 174

Message Details:

#### CRLC AM Channel Release CNF

RLC LLA @ 00:00:50.290

BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 174

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:00:50.300

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:3

#### CRLC_Config_REQ

RRC LLA @ 00:00:50.300

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:4

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC AM Channel Release REQ

LLA RLC @ 00:00:50.300

BTS unit: 1:1
Channel No: 4 Name: DCCH
CFN: 175

Message Details:

#### CRLC AM Channel Release CNF

RLC LLA @ 00:00:50.310

BTS unit: 1:1
Channel No: 4 Name: DCCH
CFN: 176

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:00:50.320

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:4

#### CRLC_Config_REQ

RRC LLA @ 00:00:50.320

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:1

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode)

dl_UM_RLC_Mode:

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):136

dl_RLCModeInfo: (UL_RLC_Mode)

ul_UM_RLC_Mode:

transmissionRLC_Discard:

timerBasedNoExplicit (NoExplicitDiscard):dt100

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity):1
dLlogicalChannelIdentity (LogicalChannelIdentity):1
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC UM Channel Establish REQ

LLA RLC @ 00:00:50.320

BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 177

Message Details:

Configuration Parameters:

PU Size In Bits:136

#### CRLC UM Channel Establish CNF

RLC LLA @ 00:00:50.320

BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 177

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:00:50.330

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:1

#### CRLC_Config_REQ

RRC LLA @ 00:00:50.330

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:2

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode)

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):128

dl_RLCModeInfo: (UL_RLC_Mode)

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity):2
dLlogicalChannelIdentity (LogicalChannelIdentity):2
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC AM Channel Establish REQ

LLA RLC @ 00:00:50.340

BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 179

Message Details:

Configuration Parameters:

PU Size In Bits:128

Timer Parameters:

Poll (ms):200
Poll Prohibit (ms):0
EPC (ms):0
Discard (ms):0
Poll Periodic (ms):0
Status Prohibit (ms):0
Status Periodic (ms):0
Reset (ms):500
MRW (ms):0

Protocol Parameters:

Max Dat:15
Poll PU:0
Poll SDU:1
Poll Window:99
Max Reset:1
Tx Window Size:32
Rx Window Size:32
Max MRW:0
SDU Discard Mode:No discard

Polling Triggers:

Last PU In Buffer:On
Last PU In Retransmission Buffer:On
Poll Timer:On
Every Poll-PU PU:Off
Every Poll-SDU SDU:On
Poll-Window Percent Of Transmission Buffer:On
Timer Based:Off

Status Triggers:

Missing PU:On
Timer Based:Off
EPC Mechanism:Off

#### CRLC AM Channel Establish CNF

RLC LLA @ 00:00:50.340

BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 179

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:00:50.350

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:2

#### CRLC_Config_REQ

RRC LLA @ 00:00:50.350

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:3

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode)

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):128

dl_RLCModeInfo: (UL_RLC_Mode)

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity):3
dLlogicalChannelIdentity (LogicalChannelIdentity):3
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC AM Channel Establish REQ

LLA RLC @ 00:00:50.350

BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 180

Message Details:

Configuration Parameters:

PU Size In Bits:128

Timer Parameters:

Poll (ms):200
Poll Prohibit (ms):0
EPC (ms):0
Discard (ms):0
Poll Periodic (ms):0
Status Prohibit (ms):0
Status Periodic (ms):0
Reset (ms):500
MRW (ms):0

Protocol Parameters:

Max Dat:15
Poll PU:0
Poll SDU:1
Poll Window:99
Max Reset:1
Tx Window Size:32
Rx Window Size:32
Max MRW:0
SDU Discard Mode:No discard

Polling Triggers:

Last PU In Buffer:On
Last PU In Retransmission Buffer:On
Poll Timer:On
Every Poll-PU PU:Off
Every Poll-SDU SDU:On
Poll-Window Percent Of Transmission Buffer:On
Timer Based:Off

Status Triggers:

Missing PU:On
Timer Based:Off
EPC Mechanism:Off

#### CRLC AM Channel Establish CNF

RLC LLA @ 00:00:50.350

BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 180

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:00:50.360

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:3

#### CRLC_Config_REQ

RRC LLA @ 00:00:50.360

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:4

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode)

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):128

dl_RLCModeInfo: (UL_RLC_Mode)

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity):4
dLlogicalChannelIdentity (LogicalChannelIdentity):4
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC AM Channel Establish REQ

LLA RLC @ 00:00:50.370

BTS unit: 1:1
Channel No: 4 Name: DCCH
CFN: 182

Message Details:

Configuration Parameters:

PU Size In Bits:128

Timer Parameters:

Poll (ms):200
Poll Prohibit (ms):0
EPC (ms):0
Discard (ms):0
Poll Periodic (ms):0
Status Prohibit (ms):0
Status Periodic (ms):0
Reset (ms):500
MRW (ms):0

Protocol Parameters:

Max Dat:15
Poll PU:0
Poll SDU:1
Poll Window:99
Max Reset:1
Tx Window Size:32
Rx Window Size:32
Max MRW:0
SDU Discard Mode:No discard

Polling Triggers:

Last PU In Buffer:On
Last PU In Retransmission Buffer:On
Poll Timer:On
Every Poll-PU PU:Off
Every Poll-SDU SDU:On
Poll-Window Percent Of Transmission Buffer:On
Timer Based:Off

Status Triggers:

Missing PU:On
Timer Based:Off
EPC Mechanism:Off

#### CRLC AM Channel Establish CNF

RLC LLA @ 00:00:50.370

BTS unit: 1:1
Channel No: 4 Name: DCCH
CFN: 182

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:00:50.380

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:4

#### MMI_CmdReq

RRC LLA @ 00:00:50.380

Message Details:

MMI_CmdReq:

cmd (IA5String):Please switch on the UE

#### MMI_CmdCnf

LLA RRC @ 00:00:51.910

Message Details:

MMI_CmdCnf:

result:true
resultString (IA5String): Omit

#### PHY_DATA_IND

PHY MAC @ 00:01:17.120

BTS unit: 1:1
Channel No: 0 Name: U_RACH
CFN: 21

Message Details:

TFI:0
TB set size:168
TB size:168
TB set (raw):

[0]08 44 48 8C D1 00 04 02
[8]00 02 C0 00 00 00 00 00
[16]00 00 00 00 00 00

TB set (decoded):

TB 0:

TCTF:0
MAC SDU (166 bits):

[0]21 11 22 33 44 00 10 08
[8]00 0B 00 00 00 00 00 00
[16]00 00 00 00 00

#### MAC_DATA_IND

MAC RLC @ 00:01:17.120

Category: Configuration
BTS unit: 1:1
Channel No: 0 Name: CCCH
CFN: 21

Message Details:

RLC PDU size (bits):166
RLC PDU (raw):

[0]21 11 22 33 44 00 10 08
[8]00 0B 00 00 00 00 00 00
[16]00 00 00 00 00

#### RLC_TR_DATA_IND: rrcConnectionRequest

RLC LLA @ 00:01:17.140

Channel No: 0 Name: CCCH

Message Details:

UL_CCCH_Message:

integrityCheckInfo: Omitted

message:

rrcConnectionRequest:

initialUE_Identity:

tmsi_and_LAI:

tmsi: 00010001001000100011001101000100

lai:

plmn_Identity:

mcc:

MCC.element: 0

MCC.element: 0

MCC.element: 1

mnc:

MNC.element: 0

MNC.element: 1

lac: 0000000000000001

establishmentCause: registration_EstablishmentCause [enum=12]

protocolErrorIndicator: noError_ProtocolErrorIndicator [enum=0]

measuredResultsOnRACH: Omitted

v3d0NonCriticalExtensions: Omitted

Layer 3 SDU:

[0]21 11 22 33 44 00 10 08
[8]00 0B 00 00 00 00 00 00
[16]00 00 00 00 00

#### RLC_TR_DATA_IND

LLA RRC @ 00:01:17.140

Channel ID: Rb0
Cell ID: 0

Message Details:

RLC_TR_DATA_IND:

cellId:0

routingInfo:

rB_Identity:0

tM_message:

uL_CCCH_Message:

integrityCheckInfo: Omit

message: (UL_CCCH_MessageType)

rrcConnectionRequest:

initialUE_Identity:

tmsi_and_LAI: (TMSI_and_LAI_GSM_MAP)

tmsi (TMSI_GSM_MAP):00010001001000100011001101000100

lai:

plmn_Identity:

mcc:

Digit:0
Digit:0
Digit:1

mnc:

Digit:0
Digit:1

lac:0000000000000001

establishmentCause:registration
protocolErrorIndicator:noError

measuredResultsOnRACH: Omit

v3d0NonCriticalExtensions: Omit

#### RLC_UM_DATA_REQ

RRC LLA @ 00:01:17.140

Channel ID: Rb0
Cell ID: 0

Message Details:

RLC_UM_DATA_REQ:

cellId:0

routingInfo:

rB_Identity:0

uM_message:

dL_CCCH_Message:

integrityCheckInfo: Omit

message: (DL_CCCH_MessageType)

rrcConnectionSetup:

r3:

rrcConnectionSetup_r3: (RRCConnectionSetup_r3_IEs)

initialUE_Identity:

tmsi_and_LAI: (TMSI_and_LAI_GSM_MAP)

tmsi (TMSI_GSM_MAP):00010001001000100011001101000100

lai:

plmn_Identity:

mcc:

Digit:0
Digit:0
Digit:1

mnc:

Digit:0
Digit:1

lac:0000000000000001

rrc_TransactionIdentifier:0
activationTime: Omit

new_U_RNTI: (U_RNTI)

srnc_Identity:000000000001
s_RNTI:00000000000000000001

new_c_RNTI (C_RNTI): Omit
rrc_StateIndicator:cell_DCH
utran_DRX_CycleLengthCoeff (UTRAN_DRX_CycleLengthCoefficient):9

capabilityUpdateRequirement:

ue_RadioCapabilityFDDUpdateRequirement:true
ue_RadioCapabilityTDDUpdateRequirement:false

systemSpecificCapUpdateReqList:

SystemSpecificCapUpdateReq:gsm

srb_InformationSetupList: (SRB_InformationSetupList2)

SRB_InformationSetup:

rb_Identity: Omit

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_UM_RLC_Mode:

transmissionRLC_Discard: Omit

dl_RLC_Mode:

dl_UM_RLC_Mode:

rb_MappingInfo:

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

dch (TransportChannelIdentity):5

logicalChannelIdentity:1

rlc_SizeList:

configured:

mac_LogicalChannelPriority:1

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

dch (TransportChannelIdentity):10

logicalChannelIdentity:1

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

rach:

logicalChannelIdentity:1

rlc_SizeList:

explicitList: (RLC_SizeExplicitList)

RLC_SizeInfo:

rlc_SizeIndex:1

mac_LogicalChannelPriority:1

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

fach:

logicalChannelIdentity:1

SRB_InformationSetup:

rb_Identity: Omit

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

rb_MappingInfo:

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

dch (TransportChannelIdentity):5

logicalChannelIdentity:2

rlc_SizeList:

configured:

mac_LogicalChannelPriority:2

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

dch (TransportChannelIdentity):10

logicalChannelIdentity:2

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

rach:

logicalChannelIdentity:2

rlc_SizeList:

explicitList: (RLC_SizeExplicitList)

RLC_SizeInfo:

rlc_SizeIndex:1

mac_LogicalChannelPriority:2

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

fach:

logicalChannelIdentity:2

SRB_InformationSetup:

rb_Identity: Omit

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

rb_MappingInfo:

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

dch (TransportChannelIdentity):5

logicalChannelIdentity:3

rlc_SizeList:

configured:

mac_LogicalChannelPriority:3

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

dch (TransportChannelIdentity):10

logicalChannelIdentity:3

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

rach:

logicalChannelIdentity:3

rlc_SizeList:

explicitList: (RLC_SizeExplicitList)

RLC_SizeInfo:

rlc_SizeIndex:1

mac_LogicalChannelPriority:3

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

fach:

logicalChannelIdentity:3

SRB_InformationSetup:

rb_Identity: Omit

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

rb_MappingInfo:

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

dch (TransportChannelIdentity):5

logicalChannelIdentity:4

rlc_SizeList:

configured:

mac_LogicalChannelPriority:4

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

dch (TransportChannelIdentity):10

logicalChannelIdentity:4

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

rach:

logicalChannelIdentity:4

rlc_SizeList:

explicitList: (RLC_SizeExplicitList)

RLC_SizeInfo:

rlc_SizeIndex:1

mac_LogicalChannelPriority:4

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

fach:

logicalChannelIdentity:4

ul_CommonTransChInfo:

tfc_Subset: Omit

prach_TFCS: (TFCS) Omit

modeSpecificInfo:

fdd:

ul_TFCS: (TFCS)

normalTFCI_Signalling: (ExplicitTFCS_Configuration)

complete: (TFCS_ReconfAdd)

ctfcSize:

ctfc2Bit:

:

ctfc2:0

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc2:1

powerOffsetInformation:

gainFactorInformation:

signalledGainFactors:

modeSpecificInfo:

fdd:

gainFactorBetaC (GainFactor):11

gainFactorBetaD (GainFactor):15
referenceTFC_ID:0

powerOffsetPp_m: Omit

ul_AddReconfTransChInfoList:

UL_AddReconfTransChInformation:

ul_TransportChannelType (UL_TrCH_Type):dch
transportChannelIdentity:5

transportFormatSet:

dedicatedTransChTFS:

tti:

tti10: (DedicatedDynamicTF_InfoList)

DedicatedDynamicTF_Info:

rlc_Size:

bitMode: (BitModeRLC_SizeInfo)

sizeType2:

part1:2
part2: Omit

numberOfTbSizeList:

NumberOfTransportBlocks:

zero:

NumberOfTransportBlocks:

one:

logicalChannelList:

allSizes:

semistaticTF_Information:

channelCodingType:

convolutional (CodingRate):third

rateMatchingAttribute:192
crc_Size:crc16

dl_CommonTransChInfo:

sccpch_TFCS: (TFCS) Omit

modeSpecificInfo:

fdd:

dl_Parameters:

sameAsUL:

dl_AddReconfTransChInfoList:

DL_AddReconfTransChInformation:

dl_TransportChannelType (DL_TrCH_Type):dch
dl_transportChannelIdentity (TransportChannelIdentity):10

tfs_SignallingMode:

sameAsULTrCH: (UL_TransportChannelIdentity)

ul_TransportChannelType (UL_TrCH_Type):dch
ul_TransportChannelIdentity (TransportChannelIdentity):5

dch_QualityTarget: (QualityTarget)

bler_QualityValue:-20

dummy: (TM_SignallingInfo) Omit

frequencyInfo: Omit

maxAllowedUL_TX_Power: Omit

ul_ChannelRequirement:

ul_DPCH_Info:

ul_DPCH_PowerControlInfo:

fdd:

dpcch_PowerOffset:-40
pc_Preamble:1
sRB_delay:7

powerControlAlgorithm:

algorithm1 (TPC_StepSizeFDD):0

modeSpecificInfo:

fdd:

scramblingCodeType:longSC
scramblingCode (UL_ScramblingCode):0
numberOfDPDCH: Omit
spreadingFactor:sf64
tfci_Existence:true
numberOfFBI_Bits: Omit
puncturingLimit:pl1

dl_CommonInformation:

dl_DPCH_InfoCommon:

cfnHandling:

initialise:

cfntargetsfnframeoffset: Omit

modeSpecificInfo:

fdd:

dl_DPCH_PowerControlInfo:

modeSpecificInfo:

fdd:

dpc_Mode:singleTPC

powerOffsetPilot_pdpdch:0

dl_rate_matching_restriction: Omit

spreadingFactorAndPilot: (SF512_AndPilot)

sfd128 (PilotBits128):pb4

positionFixedOrFlexible:fixed
tfci_Existence:false

modeSpecificInfo:

fdd:

defaultDPCH_OffsetValue (DefaultDPCH_OffsetValueFDD):0

dpch_CompressedModeInfo: Omit

tx_DiversityMode:noDiversity

ssdt_Information: Omit

dl_InformationPerRL_List:

DL_InformationPerRL:

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode:100

pdsch_SHO_DCH_Info: Omit

pdsch_CodeMapping: Omit

dl_DPCH_InfoPerRL:

fdd:

pCPICH_UsageForChannelEst:mayBeUsed
dpch_FrameOffset:0

secondaryCPICH_Info: Omit

dl_ChannelisationCodeList:

DL_ChannelisationCode:

secondaryScramblingCode:1

sf_AndCodeNumber: (SF512_AndCodeNumber)

sf128:0

scramblingCodeChange:noCodeChange

tpc_CombinationIndex:0
ssdt_CellIdentity: Omit
closedLoopTimingAdjMode: Omit

sccpch_InfoforFACH: Omit

laterNonCriticalExtensions: Omit

specialLI:true

#### RLC_UM_DATA_REQ: rrcConnectionSetup

LLA RLC @ 00:01:17.160

Channel No: 1 Name: CCCH

Message Details:

DL_CCCH_Message:

integrityCheckInfo: Omitted

message:

rrcConnectionSetup:

r3:

rrcConnectionSetup_r3:

initialUE_Identity:

tmsi_and_LAI:

tmsi: 00010001001000100011001101000100

lai:

plmn_Identity:

mcc:

MCC.element: 0

MCC.element: 0

MCC.element: 1

mnc:

MNC.element: 0

MNC.element: 1

lac: 0000000000000001

rrc_TransactionIdentifier: 0

activationTime: Omitted

new_U_RNTI:

srnc_Identity: 000000000001

s_RNTI: 00000000000000000001

new_c_RNTI: Omitted

rrc_StateIndicator: cell_DCH_RRC_StateIndicator [enum=0]

utran_DRX_CycleLengthCoeff: 9

capabilityUpdateRequirement:

ue_RadioCapabilityFDDUpdateRequirement: 1

ue_RadioCapabilityTDDUpdateRequirement: 0

systemSpecificCapUpdateReqList:

SystemSpecificCapUpdateReqList.element: gsm_SystemSpecificCapUpdateReq [enum=0]

srb_InformationSetupList:

SRB_InformationSetupList2.element:

rb_Identity: Omitted

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_UM_RLC_Mode:

transmissionRLC_Discard: Omitted

dl_RLC_Mode:

dl_UM_RLC_Mode: NULL

rb_MappingInfo:

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

dch: 5

logicalChannelIdentity: 1

rlc_SizeList:

configured: NULL

mac_LogicalChannelPriority: 1

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

dch: 10

logicalChannelIdentity: 1

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

rach: NULL

logicalChannelIdentity: 1

rlc_SizeList:

explicitList:

RLC_SizeExplicitList.element:

rlc_SizeIndex: 1

mac_LogicalChannelPriority: 1

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

fach: NULL

logicalChannelIdentity: 1

SRB_InformationSetupList2.element:

rb_Identity: Omitted

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard: dat15_MaxDAT [enum=10]

transmissionWindowSize: tw32_TransmissionWindowSize [enum=3]

timerRST: tr500_TimerRST [enum=9]

max_RST: rst1_MaxRST [enum=0]

pollingInfo:

timerPollProhibit: tpp200_TimerPollProhibit [enum=19]

timerPoll: tp200_TimerPoll [enum=19]

poll_PDU: Omitted

poll_SDU: sdu1_Poll_SDU [enum=0]

lastTransmissionPDU_Poll: 1

lastRetransmissionPDU_Poll: 1

pollWindow: pw99_PollWindow [enum=7]

timerPollPeriodic: Omitted

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery: 1

receivingWindowSize: rw32_ReceivingWindowSize [enum=3]

dl_RLC_StatusInfo:

timerStatusProhibit: tsp200_TimerStatusProhibit [enum=19]

timerEPC: Omitted

missingPDU_Indicator: 1

timerStatusPeriodic: Omitted

rb_MappingInfo:

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

dch: 5

logicalChannelIdentity: 2

rlc_SizeList:

configured: NULL

mac_LogicalChannelPriority: 2

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

dch: 10

logicalChannelIdentity: 2

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

rach: NULL

logicalChannelIdentity: 2

rlc_SizeList:

explicitList:

RLC_SizeExplicitList.element:

rlc_SizeIndex: 1

mac_LogicalChannelPriority: 2

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

fach: NULL

logicalChannelIdentity: 2

SRB_InformationSetupList2.element:

rb_Identity: Omitted

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard: dat15_MaxDAT [enum=10]

transmissionWindowSize: tw32_TransmissionWindowSize [enum=3]

timerRST: tr500_TimerRST [enum=9]

max_RST: rst1_MaxRST [enum=0]

pollingInfo:

timerPollProhibit: tpp200_TimerPollProhibit [enum=19]

timerPoll: tp200_TimerPoll [enum=19]

poll_PDU: Omitted

poll_SDU: sdu1_Poll_SDU [enum=0]

lastTransmissionPDU_Poll: 1

lastRetransmissionPDU_Poll: 1

pollWindow: pw99_PollWindow [enum=7]

timerPollPeriodic: Omitted

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery: 1

receivingWindowSize: rw32_ReceivingWindowSize [enum=3]

dl_RLC_StatusInfo:

timerStatusProhibit: tsp200_TimerStatusProhibit [enum=19]

timerEPC: Omitted

missingPDU_Indicator: 1

timerStatusPeriodic: Omitted

rb_MappingInfo:

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

dch: 5

logicalChannelIdentity: 3

rlc_SizeList:

configured: NULL

mac_LogicalChannelPriority: 3

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

dch: 10

logicalChannelIdentity: 3

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

rach: NULL

logicalChannelIdentity: 3

rlc_SizeList:

explicitList:

RLC_SizeExplicitList.element:

rlc_SizeIndex: 1

mac_LogicalChannelPriority: 3

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

fach: NULL

logicalChannelIdentity: 3

SRB_InformationSetupList2.element:

rb_Identity: Omitted

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard: dat15_MaxDAT [enum=10]

transmissionWindowSize: tw32_TransmissionWindowSize [enum=3]

timerRST: tr500_TimerRST [enum=9]

max_RST: rst1_MaxRST [enum=0]

pollingInfo:

timerPollProhibit: tpp200_TimerPollProhibit [enum=19]

timerPoll: tp200_TimerPoll [enum=19]

poll_PDU: Omitted

poll_SDU: sdu1_Poll_SDU [enum=0]

lastTransmissionPDU_Poll: 1

lastRetransmissionPDU_Poll: 1

pollWindow: pw99_PollWindow [enum=7]

timerPollPeriodic: Omitted

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery: 1

receivingWindowSize: rw32_ReceivingWindowSize [enum=3]

dl_RLC_StatusInfo:

timerStatusProhibit: tsp200_TimerStatusProhibit [enum=19]

timerEPC: Omitted

missingPDU_Indicator: 1

timerStatusPeriodic: Omitted

rb_MappingInfo:

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

dch: 5

logicalChannelIdentity: 4

rlc_SizeList:

configured: NULL

mac_LogicalChannelPriority: 4

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

dch: 10

logicalChannelIdentity: 4

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

rach: NULL

logicalChannelIdentity: 4

rlc_SizeList:

explicitList:

RLC_SizeExplicitList.element:

rlc_SizeIndex: 1

mac_LogicalChannelPriority: 4

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

fach: NULL

logicalChannelIdentity: 4

ul_CommonTransChInfo:

tfc_Subset: Omitted

prach_TFCS: Omitted

modeSpecificInfo:

fdd:

ul_TFCS:

normalTFCI_Signalling:

complete:

ctfcSize:

ctfc2Bit:

ctfc2Bit.noName:

ctfc2: 0

powerOffsetInformation:

gainFactorInformation:

computedGainFactors: 0

powerOffsetPp_m: Omitted

ctfc2Bit.noName:

ctfc2: 1

powerOffsetInformation:

gainFactorInformation:

signalledGainFactors:

modeSpecificInfo:

fdd:

gainFactorBetaC: 11

gainFactorBetaD: 15

referenceTFC_ID: 0

powerOffsetPp_m: Omitted

ul_AddReconfTransChInfoList:

UL_AddReconfTransChInfoList.element:

ul_TransportChannelType: dch_UL_TrCH_Type [enum=0]

transportChannelIdentity: 5

transportFormatSet:

dedicatedTransChTFS:

tti:

tti10:

DedicatedDynamicTF_InfoList.element:

rlc_Size:

bitMode:

sizeType2:

part1: 2

part2: Omitted

numberOfTbSizeList:

numberOfTbSizeList.element:

zero: NULL

numberOfTbSizeList.element:

one: NULL

logicalChannelList:

allSizes: NULL

semistaticTF_Information:

channelCodingType:

convolutional: third_CodingRate [enum=1]

rateMatchingAttribute: 192

crc_Size: crc16_CRC_Size [enum=3]

dl_CommonTransChInfo:

sccpch_TFCS: Omitted

modeSpecificInfo:

fdd:

dl_Parameters:

sameAsUL: NULL

dl_AddReconfTransChInfoList:

DL_AddReconfTransChInfoList.element:

dl_TransportChannelType: dch_DL_TrCH_Type [enum=0]

dl_transportChannelIdentity: 10

tfs_SignallingMode:

sameAsULTrCH:

ul_TransportChannelType: dch_UL_TrCH_Type [enum=0]

ul_TransportChannelIdentity: 5

dch_QualityTarget:

bler_QualityValue: -20

dummy: Omitted

frequencyInfo: Omitted

maxAllowedUL_TX_Power: Omitted

ul_ChannelRequirement:

ul_DPCH_Info:

ul_DPCH_PowerControlInfo:

fdd:

dpcch_PowerOffset: -40

pc_Preamble: 1

sRB_delay: 7

powerControlAlgorithm:

algorithm1: 0

modeSpecificInfo:

fdd:

scramblingCodeType: longSC_ScramblingCodeType [enum=1]

scramblingCode: 0

numberOfDPDCH: Default

spreadingFactor: sf64_SpreadingFactor [enum=4]

tfci_Existence: 1

numberOfFBI_Bits: Omitted

puncturingLimit: pl1_PuncturingLimit [enum=15]

dl_CommonInformation:

dl_DPCH_InfoCommon:

cfnHandling:

initialise:

cfntargetsfnframeoffset: Omitted

modeSpecificInfo:

fdd:

dl_DPCH_PowerControlInfo:

modeSpecificInfo:

fdd:

dpc_Mode: singleTPC_DPC_Mode [enum=0]

powerOffsetPilot_pdpdch: 0

dl_rate_matching_restriction: Omitted

spreadingFactorAndPilot:

sfd128: pb4_PilotBits128 [enum=0]

positionFixedOrFlexible: fixed_PositionFixedOrFlexible [enum=0]

tfci_Existence: 0

modeSpecificInfo:

fdd:

defaultDPCH_OffsetValue: 0

dpch_CompressedModeInfo: Omitted

tx_DiversityMode: noDiversity_TX_DiversityMode [enum=0]

ssdt_Information: Omitted

dl_InformationPerRL_List:

DL_InformationPerRL_List.element:

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode: 100

pdsch_SHO_DCH_Info: Omitted

pdsch_CodeMapping: Omitted

dl_DPCH_InfoPerRL:

fdd:

pCPICH_UsageForChannelEst: mayBeUsed_PCPICH_UsageForChannelEst [enum=0]

dpch_FrameOffset: 0

secondaryCPICH_Info: Omitted

dl_ChannelisationCodeList:

DL_ChannelisationCodeList.element:

secondaryScramblingCode: 1

sf_AndCodeNumber:

sf128: 0

scramblingCodeChange: noCodeChange_ScramblingCodeChange [enum=1]

tpc_CombinationIndex: 0

ssdt_CellIdentity: Omitted

closedLoopTimingAdjMode: Omitted

sccpch_InfoforFACH: Omitted

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]30 E7 22 24 46 68 80 02
[8]01 00 01 00 04 00 00 4D
[16]82 69 3A 10 10 89 0D 42
[24]00 02 81 9E 8E 46 C9 A6
[32]7C 9C 4E 74 20 A5 12 3A
[40]8C 00 15 13 3D 1C 8D 93
[48]4C F9 38 9C E8 42 52 24
[56]B5 28 00 4A 46 7A 39 1B
[64]26 99 F2 71 39 D0 86 B4
[72]49 EA 70 00 D4 C8 00 06
[80]25 2B F0 02 00 08 82 23
[88]BF 66 08 98 95 A5 47 82
[96]00 00 01 3F 90 0A 14 00
[104]02 06 40 00 0C 28 08

#### MAC_DATA_REQ

RLC MAC @ 00:01:17.190

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: CCCH
CFN: 48

Message Details:

RLC PDU size (bits):160
RLC PDU (raw):

[0]19 F8 30 E7 22 24 46 68
[8]80 02 01 00 01 00 04 00
[16]00 4D 82 69

RLC PDU (decoded):

Sequence number:12
Length indicator 0 (octets):124 (the first data octet in this RLC PDU is the first octet of a RLC SDU)
Segment associated with length indicator 0 (0 octets):

Last segment, not associated with any length indicators (18 octets):

[0]30 E7 22 24 46 68 80 02
[8]01 00 01 00 04 00 00 4D
[16]82 69

#### MAC_DATA_REQ

RLC MAC @ 00:01:17.190

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: CCCH
CFN: 48

Message Details:

RLC PDU size (bits):160
RLC PDU (raw):

[0]1A 3A 10 10 89 0D 42 00
[8]02 81 9E 8E 46 C9 A6 7C
[16]9C 4E 74 20

RLC PDU (decoded):

Sequence number:13
Last segment, not associated with any length indicators (19 octets):

[0]3A 10 10 89 0D 42 00 02
[8]81 9E 8E 46 C9 A6 7C 9C
[16]4E 74 20

#### MAC_DATA_REQ

RLC MAC @ 00:01:17.190

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: CCCH
CFN: 48

Message Details:

RLC PDU size (bits):160
RLC PDU (raw):

[0]1C A5 12 3A 8C 00 15 13
[8]3D 1C 8D 93 4C F9 38 9C
[16]E8 42 52 24

RLC PDU (decoded):

Sequence number:14
Last segment, not associated with any length indicators (19 octets):

[0]A5 12 3A 8C 00 15 13 3D
[8]1C 8D 93 4C F9 38 9C E8
[16]42 52 24

#### MAC_DATA_REQ

RLC MAC @ 00:01:17.190

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: CCCH
CFN: 48

Message Details:

RLC PDU size (bits):160
RLC PDU (raw):

[0]1E B5 28 00 4A 46 7A 39
[8]1B 26 99 F2 71 39 D0 86
[16]B4 49 EA 70

RLC PDU (decoded):

Sequence number:15
Last segment, not associated with any length indicators (19 octets):

[0]B5 28 00 4A 46 7A 39 1B
[8]26 99 F2 71 39 D0 86 B4
[16]49 EA 70

#### MAC_DATA_REQ

RLC MAC @ 00:01:17.190

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: CCCH
CFN: 48

Message Details:

RLC PDU size (bits):160
RLC PDU (raw):

[0]20 00 D4 C8 00 06 25 2B
[8]F0 02 00 08 82 23 BF 66
[16]08 98 95 A5

RLC PDU (decoded):

Sequence number:16
Last segment, not associated with any length indicators (19 octets):

[0]00 D4 C8 00 06 25 2B F0
[8]02 00 08 82 23 BF 66 08
[16]98 95 A5

#### MAC_DATA_REQ

RLC MAC @ 00:01:17.190

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: CCCH
CFN: 48

Message Details:

RLC PDU size (bits):160
RLC PDU (raw):

[0]23 23 FE 47 82 00 00 01
[8]3F 90 0A 14 00 02 06 40
[16]00 0C 28 08

RLC PDU (decoded):

Sequence number:17
Length indicator 0 (octets):17
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (17 octets):

[0]47 82 00 00 01 3F 90 0A
[8]14 00 02 06 40 00 0C 28
[16]08
Padding associated with length indicator 1 (0 octets):

#### PHY_DATA_REQ

MAC PHY @ 00:01:17.190

BTS unit: 1:1
Channel No: 0 Name: FACH
CFN: 48

Message Details:

TFI:2
TB set size:336
TB size:168
TB set (raw, each TB word aligned):

[0]40 19 F8 30 E7 22 24 46
[8]68 80 02 01 00 01 00 04
[16]00 00 4D 82 69 00 40 1A
[24]3A 10 10 89 0D 42 00 02
[32]81 9E 8E 46 C9 A6 7C 9C
[40]4E 74 20 00

TB set (decoded):

TB 0:

TCTF:64
MAC SDU (160 bits):

[0]19 F8 30 E7 22 24 46 68
[8]80 02 01 00 01 00 04 00
[16]00 4D 82 69

TB 1:

TCTF:64
MAC SDU (160 bits):

[0]1A 3A 10 10 89 0D 42 00
[8]02 81 9E 8E 46 C9 A6 7C
[16]9C 4E 74 20

#### PHY_DATA_REQ

MAC PHY @ 00:01:17.200

BTS unit: 1:1
Channel No: 0 Name: FACH
CFN: 49

Message Details:

TFI:2
TB set size:336
TB size:168
TB set (raw, each TB word aligned):

[0]40 1C A5 12 3A 8C 00 15
[8]13 3D 1C 8D 93 4C F9 38
[16]9C E8 42 52 24 00 40 1E
[24]B5 28 00 4A 46 7A 39 1B
[32]26 99 F2 71 39 D0 86 B4
[40]49 EA 70 00

TB set (decoded):

TB 0:

TCTF:64
MAC SDU (160 bits):

[0]1C A5 12 3A 8C 00 15 13
[8]3D 1C 8D 93 4C F9 38 9C
[16]E8 42 52 24

TB 1:

TCTF:64
MAC SDU (160 bits):

[0]1E B5 28 00 4A 46 7A 39
[8]1B 26 99 F2 71 39 D0 86
[16]B4 49 EA 70

#### PHY_DATA_REQ

MAC PHY @ 00:01:17.210

BTS unit: 1:1
Channel No: 0 Name: FACH
CFN: 50

Message Details:

TFI:2
TB set size:336
TB size:168
TB set (raw, each TB word aligned):

[0]40 20 00 D4 C8 00 06 25
[8]2B F0 02 00 08 82 23 BF
[16]66 08 98 95 A5 00 40 23
[24]23 FE 47 82 00 00 01 3F
[32]90 0A 14 00 02 06 40 00
[40]0C 28 08 00

TB set (decoded):

TB 0:

TCTF:64
MAC SDU (160 bits):

[0]20 00 D4 C8 00 06 25 2B
[8]F0 02 00 08 82 23 BF 66
[16]08 98 95 A5

TB 1:

TCTF:64
MAC SDU (160 bits):

[0]23 23 FE 47 82 00 00 01
[8]3F 90 0A 14 00 02 06 40
[16]00 0C 28 08

#### CPHY_SYNC_IND

PHY RRC @ 00:01:17.430

BTS unit: 1:1
Channel No: 0 Name: U_DPCH
CFN: 72

Message Details:

#### PHY_DATA_IND

PHY MAC @ 00:01:17.590

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 68

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 00 04 B0 C0 00 08 00
[8]00 51 1B 8D D0 6A 4C 66
[16]88 A2 C0 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 00 4B 0C 00 00 80 00
[8]05 11 B8 DD 06 A4 C6 68
[16]8A 2C

#### MAC_DATA_IND

MAC RLC @ 00:01:17.590

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 68

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 00 4B 0C 00 00 80 00
[8]05 11 B8 DD 06 A4 C6 68
[16]8A 2C

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:0
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]4B 0C 00 00 80 00 05 11
[8]B8 DD 06 A4 C6 68 8A 2C

#### PHY_DATA_IND

PHY MAC @ 00:01:17.600

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 69

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 00 88 30 34 80 01 80
[8]01 18 FC FC 0C C0 D5 C6
[16]28 48 C0 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 08 83 03 48 00 18 00
[8]11 8F CF C0 CC 0D 5C 62
[16]84 8C

#### MAC_DATA_IND

MAC RLC @ 00:01:17.600

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 69

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 08 83 03 48 00 18 00
[8]11 8F CF C0 CC 0D 5C 62
[16]84 8C

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:1
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]83 03 48 00 18 00 11 8F
[8]CF C0 CC 0D 5C 62 84 8C

#### PHY_DATA_IND

PHY MAC @ 00:01:17.610

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 70

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 01 50 BF E0 28 99 01
[8]00 05 55 55 55 55 55 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 15 0B FE 02 89 90 10
[8]00 55 55 55 55 55 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:01:17.610

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 70

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 15 0B FE 02 89 90 10
[8]00 55 55 55 55 55 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:2
Polling bit:1 (request a status report)
Length indicator 0 (octets):5
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (5 octets):

[0]02 89 90 10 00
Padding associated with length indicator 1 (9 octets):

[0]55 55 55 55 55 55 55 55
[8]55

#### MAC_DATA_REQ

RLC MAC @ 00:01:17.620

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 91

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:3

#### PHY_DATA_REQ

MAC PHY @ 00:01:17.620

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 91

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]10 20 03 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:01:17.620

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 71

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 00 01 58 0D 10 10 84
[8]00 81 72 A0 01 83 82 02
[16]FA 09 10 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 00 15 80 D1 01 08 40
[8]08 17 2A 00 18 38 20 2F
[16]A0 91

#### MAC_DATA_IND

MAC RLC @ 00:01:17.620

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 71

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 00 15 80 D1 01 08 40
[8]08 17 2A 00 18 38 20 2F
[16]A0 91

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:0
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]15 80 D1 01 08 40 08 17
[8]2A 00 18 38 20 2F A0 91

#### PHY_DATA_IND

PHY MAC @ 00:01:17.630

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 72

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 00 8A 2B 3C 00 78 88
[8]00 00 82 85 8A F9 C1 19
[16]AA 15 10 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 08 A2 B3 C0 07 88 80
[8]00 08 28 58 AF 9C 11 9A
[16]A1 51

#### MAC_DATA_IND

MAC RLC @ 00:01:17.630

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 72

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 08 A2 B3 C0 07 88 80
[8]00 08 28 58 AF 9C 11 9A
[16]A1 51

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:1
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]A2 B3 C0 07 88 80 00 08
[8]28 58 AF 9C 11 9A A1 51

#### RLC_AM_DATA_IND: rrcConnectionSetupComplete

RLC LLA @ 00:01:17.630

Channel No: 2 Name: DCCH

Message Details:

UL_DCCH_Message:

integrityCheckInfo: Omitted

message:

rrcConnectionSetupComplete:

rrc_TransactionIdentifier: 0

startList:

STARTList.element:

cn_DomainIdentity: ps_domain_CN_DomainIdentity [enum=1]

start_Value: 00000000000000000010

STARTList.element:

cn_DomainIdentity: cs_domain_CN_DomainIdentity [enum=0]

start_Value: 00000000000000000010

ue_RadioAccessCapability:

accessStratumReleaseIndicator: r99_AccessStratumReleaseIndicator [enum=0]

pdcp_Capability:

losslessSRNS_RelocationSupport: 0

supportForRfc2507:

notSupported: NULL

rlc_Capability:

totalRLC_AM_BufferSize: kb50_TotalRLC_AM_BufferSize [enum=2]

maximumRLC_WindowSize: mws2047_MaximumRLC_WindowSize [enum=0]

maximumAM_EntityNumber: am6_MaximumAM_EntityNumberRLC_Cap [enum=3]

transportChannelCapability:

dl_TransChCapability:

maxNoBitsReceived: b8960_MaxNoBits [enum=7]

maxConvCodeBitsReceived: b1280_MaxNoBits [enum=1]

turboDecodingSupport:

supported: b8960_MaxNoBits [enum=7]

maxSimultaneousTransChs: e8_MaxSimultaneousTransChsDL [enum=1]

maxSimultaneousCCTrCH_Count: 1

maxReceivedTransportBlocks: tb32_MaxTransportBlocksDL [enum=3]

maxNumberOfTFC: tfc128_MaxNumberOfTFC_DL [enum=5]

maxNumberOfTF: tf64_MaxNumberOfTF [enum=1]

ul_TransChCapability:

maxNoBitsTransmitted: b3840_MaxNoBits [enum=3]

maxConvCodeBitsTransmitted: b1280_MaxNoBits [enum=1]

turboEncodingSupport:

supported: b3840_MaxNoBits [enum=3]

maxSimultaneousTransChs: e8_MaxSimultaneousTransChsUL [enum=2]

modeSpecificInfo:

fdd: NULL

maxTransmittedBlocks: tb32_MaxTransportBlocksUL [enum=4]

maxNumberOfTFC: tfc64_MaxNumberOfTFC_UL [enum=5]

maxNumberOfTF: tf32_MaxNumberOfTF [enum=0]

rf_Capability:

fddRF_Capability:

ue_PowerClass: 4

txRxFrequencySeparation: mhz190_TxRxFrequencySeparation [enum=0]

tddRF_Capability: Omitted

physicalChannelCapability:

fddPhysChCapability:

downlinkPhysChCapability:

maxNoDPCH_PDSCH_Codes: 1

maxNoPhysChBitsReceived: b9600_MaxNoPhysChBitsReceived [enum=6]

supportForSF_512: 0

supportOfPDSCH: 0

simultaneousSCCPCH_DPCH_Reception:

notSupported: NULL

uplinkPhysChCapability:

maxNoDPDCH_BitsTransmitted: b4800_MaxNoDPDCH_BitsTransmitted [enum=3]

supportOfPCPCH: 0

tddPhysChCapability: Omitted

ue_MultiModeRAT_Capability:

multiRAT_CapabilityList:

supportOfGSM: 1

supportOfMulticarrier: 0

multiModeCapability: fdd_MultiModeCapability [enum=1]

securityCapability:

cipheringAlgorithmCap: 0000000000000011

integrityProtectionAlgorithmCap: 0000000000000010

ue_positioning_Capability:

standaloneLocMethodsSupported: 0

ue_BasedOTDOA_Supported: 0

networkAssistedGPS_Supported: noNetworkAssistedGPS_NetworkAssistedGPS_Supported [enum=3]

supportForUE_GPS_TimingOfCellFrames: 0

supportForIPDL: 0

measurementCapability:

downlinkCompressedMode:

fdd_Measurements: 1

tdd_Measurements: Omitted

gsm_Measurements:

gsm900: 1

dcs1800: 1

gsm1900: 1

multiCarrierMeasurements: 0

uplinkCompressedMode:

fdd_Measurements: 1

tdd_Measurements: Omitted

gsm_Measurements:

gsm900: 1

dcs1800: 1

gsm1900: 1

multiCarrierMeasurements: 0

ue_RATSpecificCapability:

InterRAT_UE_RadioAccessCapabilityList.element:

gsm:

gsm_Classmark2: 33035718A1

gsm_Classmark3: 60144C8080

v370NonCriticalExtensions: Omitted

Layer 3 SDU:

[0]4B 0C 00 00 80 00 05 11
[8]B8 DD 06 A4 C6 68 8A 2C
[16]83 03 48 00 18 00 11 8F
[24]CF C0 CC 0D 5C 62 84 8C
[32]02 89 90 10 00

#### RLC_AM_DATA_IND

LLA RRC @ 00:01:17.630

Channel ID: Rb2
Cell ID: -1

Message Details:

RLC_AM_DATA_IND:

cellId:-1

routingInfo:

rB_Identity:2

integrityResult:

integrityUsed (IntegrityStatus):i_pass

aM_message:

uL_DCCH_Message:

integrityCheckInfo: Omit

message: (UL_DCCH_MessageType)

rrcConnectionSetupComplete:

rrc_TransactionIdentifier:0

startList:

STARTSingle:

cn_DomainIdentity:ps_domain
start_Value:00000000000000000010

STARTSingle:

cn_DomainIdentity:cs_domain
start_Value:00000000000000000010

ue_RadioAccessCapability:

accessStratumReleaseIndicator:r99

pdcp_Capability:

losslessSRNS_RelocationSupport:false

supportForRfc2507:

notSupported:

rlc_Capability:

totalRLC_AM_BufferSize:kb50
maximumRLC_WindowSize:mws2047
maximumAM_EntityNumber (MaximumAM_EntityNumberRLC_Cap):am6

transportChannelCapability:

dl_TransChCapability:

maxNoBitsReceived (MaxNoBits):b8960
maxConvCodeBitsReceived (MaxNoBits):b1280

turboDecodingSupport: (TurboSupport)

supported (MaxNoBits):b8960

maxSimultaneousTransChs (MaxSimultaneousTransChsDL):e8
maxSimultaneousCCTrCH_Count:1
maxReceivedTransportBlocks (MaxTransportBlocksDL):tb32
maxNumberOfTFC (MaxNumberOfTFC_DL):tfc128
maxNumberOfTF:tf64

ul_TransChCapability:

maxNoBitsTransmitted (MaxNoBits):b3840
maxConvCodeBitsTransmitted (MaxNoBits):b1280

turboEncodingSupport: (TurboSupport)

supported (MaxNoBits):b3840

maxSimultaneousTransChs (MaxSimultaneousTransChsUL):e8

modeSpecificInfo:

fdd:

maxTransmittedBlocks (MaxTransportBlocksUL):tb32
maxNumberOfTFC (MaxNumberOfTFC_UL):tfc64
maxNumberOfTF:tf32

rf_Capability:

fddRF_Capability:

ue_PowerClass:4
txRxFrequencySeparation:mhz190

tddRF_Capability: Omit

physicalChannelCapability:

fddPhysChCapability:

downlinkPhysChCapability: (DL_PhysChCapabilityFDD)

maxNoDPCH_PDSCH_Codes:1
maxNoPhysChBitsReceived:b9600
supportForSF_512:false
supportOfPDSCH:false

simultaneousSCCPCH_DPCH_Reception:

notSupported:

uplinkPhysChCapability: (UL_PhysChCapabilityFDD)

maxNoDPDCH_BitsTransmitted:b4800
supportOfPCPCH:false

tddPhysChCapability: Omit

ue_MultiModeRAT_Capability:

multiRAT_CapabilityList: (MultiRAT_Capability)

supportOfGSM:true
supportOfMulticarrier:false

multiModeCapability:fdd

securityCapability:

cipheringAlgorithmCap:0000000000000011
integrityProtectionAlgorithmCap:0000000000000010

ue_positioning_Capability:

standaloneLocMethodsSupported:false
ue_BasedOTDOA_Supported:false
networkAssistedGPS_Supported:noNetworkAssistedGPS
supportForUE_GPS_TimingOfCellFrames:false
supportForIPDL:false

measurementCapability:

downlinkCompressedMode: (CompressedModeMeasCapability)

fdd_Measurements:true
tdd_Measurements: Omit

gsm_Measurements:

gsm900:true
dcs1800:true
gsm1900:true

multiCarrierMeasurements:false

uplinkCompressedMode: (CompressedModeMeasCapability)

fdd_Measurements:true
tdd_Measurements: Omit

gsm_Measurements:

gsm900:true
dcs1800:true
gsm1900:true

multiCarrierMeasurements:false

ue_RATSpecificCapability: (InterRAT_UE_RadioAccessCapabilityList)

InterRAT_UE_RadioAccessCapability:

gsm:

gsm_Classmark2:

[0]33 03 57 18 A1
gsm_Classmark3:

[0]60 14 4C 80 80

v370NonCriticalExtensions: Omit

#### PHY_DATA_IND

PHY MAC @ 00:01:17.640

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 73

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 01 51 5F E9 93 22 50
[8]CC 0B 8B 20 00 04 05 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 15 15 FE 99 32 25 0C
[8]C0 B8 B2 00 00 40 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:01:17.640

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 73

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 15 15 FE 99 32 25 0C
[8]C0 B8 B2 00 00 40 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:2
Polling bit:1 (request a status report)
Length indicator 0 (octets):10
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (10 octets):

[0]99 32 25 0C C0 B8 B2 00
[8]00 40
Padding associated with length indicator 1 (4 octets):

[0]55 55 55 55

#### RLC_AM_DATA_IND: initialDirectTransfer

RLC RRC @ 00:01:17.650

Channel No: 3 Name: DCCH

Message Details:

UL_DCCH_Message:

integrityCheckInfo: Omitted

message:

initialDirectTransfer:

cn_DomainIdentity: ps_domain_CN_DomainIdentity [enum=1]

intraDomainNasNodeSelector:

version:

release99:

cn_Type:

gsm_Map_IDNNS:

routingbasis:

localPTMSI:

routingparameter: 0011010001

enteredparameter: 0

nas_Message: 080102E54003070405F41234567800F1100001050B15F38233542A332644A1981716

measuredResultsOnRACH: Omitted

v3a0NonCriticalExtensions:

initialDirectTransfer_v3a0ext:

start_Value: 00000000000000000010

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]15 80 D1 01 08 40 08 17
[8]2A 00 18 38 20 2F A0 91
[16]A2 B3 C0 07 88 80 00 08
[24]28 58 AF 9C 11 9A A1 51
[32]99 32 25 0C C0 B8 B2 00
[40]00 40

#### RRC_DATA_IND: gmm:attachRequest

RRC NAS @ 00:01:17.650

Cell ID: -1

Message Details:

ATTACHREQUEST:

skipIndicator: 0000

gMMProtocolDiscriminator: 1000

msgType: 00000001

msNetworkCap:

iel: 02

value: E540

gprsCiphKeySeqNo:

spare1: 0

keySeq: 000

attachType:

for: 0

type: 011

drxParameter:

splitPGcycleCode: 00000111

cnDRXcoef: 0000

splitOnCCCH: 0

nonDRXtimer: 100

ptmsiORimsi:

iel: 05

iDigit1: 1111

oddEvenInd: 0

typeOfId: 100

otherDigits: 12345678

oldRAI:

plmn: 00F110

lac: 0001

rac: 05

msRadioAccessCap:

iel: 0B

value: 15F38233542A332644A198

oldPTMSI_Signature: Omitted

readyTimer:

iei: 00010111

unit: 000

value: 10110

tmsiStatus: Omitted

#### MAC_DATA_REQ

RLC MAC @ 00:01:17.650

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 94

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:3

#### PHY_DATA_REQ

MAC PHY @ 00:01:17.650

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 94

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 03 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### RRC_DATA_REQ: gmm:authenticationAndCipheringRequest

NAS RRC @ 00:01:17.660

Cell ID: -1

Message Details:

AUTHENTICATIONANDCIPHERINGREQUEST:

skipIndicator: 0000

gMMProtocolDiscriminator: 1000

msgType: 00010010

imeisvReq:

spare1: 0

value: 000

ciphAlgorithm:

spare1: 0

algorithm: 001

acRefNo:

value: 0011

forceToStandby:

spare: 0

value: 000

authRand:

iei: 00100001

randValue: 01010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101

gprsCiphKeySeqNo:

iei: 1000

spare1: 0

keySeq: 001

aUTN:

iei: 00101000

iel: 10

aUTN: 01100110000100010000000000110011001000101101110100000000000000000101010101000100011101110110011000010001000000000011001100100010

#### RLC_AM_DATA_REQ:downlinkDirectTransfer

RRC RLC @ 00:01:17.660

Channel No: 3 Name: DCCH

Message Details:

Opt1: 0

Opt2: 0

DL_DCCH_Message:

integrityCheckInfo: Omitted

message:

downlinkDirectTransfer:

r3:

downlinkDirectTransfer_r3:

rrc_TransactionIdentifier: 0

cn_DomainIdentity: ps_domain_CN_DomainIdentity [enum=1]

nas_Message: 0812013021555555555555555555555555555555558128106611003322DD00005544776611003322

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]14 20 4E 10 24 02 60 42
[8]AA AA AA AA AA AA AA AA
[16]AA AA AA AA AA AA AA AB
[24]02 50 20 CC 22 00 66 45
[32]BA 00 00 AA 88 EE CC 22
[40]00 66 44

#### MAC_DATA_REQ

RLC MAC @ 00:01:17.680

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 97

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 00 14 20 4E 10 24 02
[8]60 42 AA AA AA AA AA AA
[16]AA AA

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:0
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]14 20 4E 10 24 02 60 42
[8]AA AA AA AA AA AA AA AA

#### MAC_DATA_REQ

RLC MAC @ 00:01:17.680

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 97

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 08 AA AA AA AA AA AA
[8]AA AB 02 50 20 CC 22 00
[16]66 45

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:1
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]AA AA AA AA AA AA AA AB
[8]02 50 20 CC 22 00 66 45

#### MAC_DATA_REQ

RLC MAC @ 00:01:17.680

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 97

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 15 17 FE BA 00 00 AA
[8]88 EE CC 22 00 66 44 00
[16]00 00

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:2
Polling bit:1 (request a status report)
Length indicator 0 (octets):11
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (11 octets):

[0]BA 00 00 AA 88 EE CC 22
[8]00 66 44
Padding associated with length indicator 1 (3 octets):

[0]00 00 00

#### PHY_DATA_REQ

MAC PHY @ 00:01:17.680

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 97

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 00 01 42 04 E1 02 40
[8]26 04 2A AA AA AA AA AA
[16]AA AA A0 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 00 14 20 4E 10 24 02
[8]60 42 AA AA AA AA AA AA
[16]AA AA

#### PHY_DATA_REQ

MAC PHY @ 00:01:17.690

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 98

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 00 8A AA AA AA AA AA
[8]AA AA B0 25 02 0C C2 20
[16]06 64 50 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 08 AA AA AA AA AA AA
[8]AA AB 02 50 20 CC 22 00
[16]66 45

#### PHY_DATA_REQ

MAC PHY @ 00:01:17.700

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 99

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 01 51 7F EB A0 00 0A
[8]A8 8E EC C2 20 06 64 40
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 15 17 FE BA 00 00 AA
[8]88 EE CC 22 00 66 44 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:01:17.820

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 91

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 01 50 BF E0 28 99 01
[8]00 05 55 55 55 55 55 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 15 0B FE 02 89 90 10
[8]00 55 55 55 55 55 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:01:17.820

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 91

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 15 0B FE 02 89 90 10
[8]00 55 55 55 55 55 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:2
Polling bit:1 (request a status report)
Length indicator 0 (octets):5
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (5 octets):

[0]02 89 90 10 00
Padding associated with length indicator 1 (9 octets):

[0]55 55 55 55 55 55 55 55
[8]55

#### MAC_DATA_REQ

RLC MAC @ 00:01:17.830

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 112

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:3

#### PHY_DATA_REQ

MAC PHY @ 00:01:17.830

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 112

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]10 20 03 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:01:17.850

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 94

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 01 51 5F E9 93 22 50
[8]CC 0B 8B 20 00 04 05 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 15 15 FE 99 32 25 0C
[8]C0 B8 B2 00 00 40 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:01:17.850

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 94

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 15 15 FE 99 32 25 0C
[8]C0 B8 B2 00 00 40 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:2
Polling bit:1 (request a status report)
Length indicator 0 (octets):10
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (10 octets):

[0]99 32 25 0C C0 B8 B2 00
[8]00 40
Padding associated with length indicator 1 (4 octets):

[0]55 55 55 55

#### MAC_DATA_REQ

RLC MAC @ 00:01:17.860

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 115

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:3

#### PHY_DATA_REQ

MAC PHY @ 00:01:17.860

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 115

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 03 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### MAC_DATA_REQ

RLC MAC @ 00:01:17.880

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 117

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 15 17 FE BA 00 00 AA
[8]88 EE CC 22 00 66 44 00
[16]00 00

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:2
Polling bit:1 (request a status report)
Length indicator 0 (octets):11
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (11 octets):

[0]BA 00 00 AA 88 EE CC 22
[8]00 66 44
Padding associated with length indicator 1 (3 octets):

[0]00 00 00

#### PHY_DATA_REQ

MAC PHY @ 00:01:17.880

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 117

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 01 51 7F EB A0 00 0A
[8]A8 8E EC C2 20 06 64 40
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 15 17 FE BA 00 00 AA
[8]88 EE CC 22 00 66 44 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:01:17.930

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 102

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 03 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### MAC_DATA_IND

MAC RLC @ 00:01:17.930

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 102

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:3

#### PHY_DATA_IND

PHY MAC @ 00:01:18.080

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 117

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 01 86 C8 06 84 09 81
[8]91 2A A2 3B B3 14 82 08
[16]80 19 90 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 18 6C 80 68 40 98 19
[8]12 AA 23 BB 31 48 20 88
[16]01 99

#### MAC_DATA_IND

MAC RLC @ 00:01:18.080

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 117

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 18 6C 80 68 40 98 19
[8]12 AA 23 BB 31 48 20 88
[16]01 99

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:3
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]6C 80 68 40 98 19 12 AA
[8]23 BB 31 48 20 88 01 99

#### PHY_DATA_IND

PHY MAC @ 00:01:18.090

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 118

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 02 50 3F E1 05 55 55
[8]55 55 55 55 55 55 55 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 25 03 FE 10 55 55 55
[8]55 55 55 55 55 55 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:01:18.090

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 118

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 25 03 FE 10 55 55 55
[8]55 55 55 55 55 55 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:4
Polling bit:1 (request a status report)
Length indicator 0 (octets):1
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (1 octets):

[0]10
Padding associated with length indicator 1 (13 octets):

[0]55 55 55 55 55 55 55 55
[8]55 55 55 55 55

#### RLC_AM_DATA_IND: uplinkDirectTransfer

RLC RRC @ 00:01:18.100

Channel No: 3 Name: DCCH

Message Details:

UL_DCCH_Message:

integrityCheckInfo: Omitted

message:

uplinkDirectTransfer:

cn_DomainIdentity: ps_domain_CN_DomainIdentity [enum=1]

nas_Message: 0813032255447766290411003322

measuredResultsOnRACH: Omitted

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]6C 80 68 40 98 19 12 AA
[8]23 BB 31 48 20 88 01 99
[16]10

#### RRC_DATA_IND: gmm:authenticationAndCipheringResponse

RRC NAS @ 00:01:18.100

Cell ID: -1

Message Details:

AUTHENTICATIONANDCIPHERINGRESPONSE:

skipIndicator: 0000

gMMProtocolDiscriminator: 1000

msgType: 00010011

spare4: 0000

acRefNo:

value: 0011

authRsp:

iei: 00100010

value: 01010101010001000111011101100110

imeisv: Omitted

authRspExt:

iei: 00101001

iel: 04

rES: 00010001000000000011001100100010

#### MAC_DATA_REQ

RLC MAC @ 00:01:18.100

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 139

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 50 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:5

#### PHY_DATA_REQ

MAC PHY @ 00:01:18.100

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 139

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 05 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 50 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### CRLC_SecurityMode_Config_REQ

RRC LLA @ 00:01:18.130

Cell ID: -1

Message Details:

CRLC_SecurityMode_Config_REQ:

cellId:-1

rlcSecurityInfo: (SecurityInfo)

cn_DomainIdentity:ps_domain
startValue (START_Value):00000000000000000000
cipheringKey: Omit
integrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
gsmCipheringKey: Omit

#### CRLC_SecurityMode_Config_REQ

RRC RLC @ 00:01:18.130

Message Details:

cellIdentity: 1

rlcSecurityInfo:

cn_DomainIdentity: ps_domain_CN_DomainIdentity

startValue: 00000000000000000000

cipheringKey: Omitted

integrityKey: 01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100

#### PHY_DATA_IND

PHY MAC @ 00:01:18.140

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 123

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 03 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### MAC_DATA_IND

MAC RLC @ 00:01:18.140

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 123

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:3

#### CRLC_SecurityMode_Config_CNF

LLA RRC @ 00:01:18.140

Cell ID: -1

Message Details:

CRLC_SecurityMode_Config_CNF:

cellId:-1

#### CRLC_SetRRC_MessageSN_REQ

RRC LLA @ 00:01:18.140

Channel ID: Rb0
Cell ID: 0

Message Details:

CRLC_SetRRC_MessageSN_REQ:

cellId:0

routingInfo:

rB_Identity:0

count_I_LSB_UL (RRC_SequenceNumber): Omit
count_I_LSB_DL (RRC_SequenceNumber):0

#### CRLC_SetRRC_MessageSN_CNF

LLA RRC @ 00:01:18.160

Channel ID: Rb0
Cell ID: 0

Message Details:

CRLC_SetRRC_MessageSN_CNF:

cellId:0

routingInfo:

rB_Identity:0

#### CRLC_SetRRC_MessageSN_REQ

RRC LLA @ 00:01:18.160

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_REQ:

cellId:-1

routingInfo:

rB_Identity:1

count_I_LSB_UL (RRC_SequenceNumber): Omit
count_I_LSB_DL (RRC_SequenceNumber):0

#### CRLC_SetRRC_MessageSN_CNF

LLA RRC @ 00:01:18.180

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_CNF:

cellId:-1

routingInfo:

rB_Identity:1

#### CRLC_SetRRC_MessageSN_REQ

RRC LLA @ 00:01:18.180

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_REQ:

cellId:-1

routingInfo:

rB_Identity:2

count_I_LSB_UL (RRC_SequenceNumber): Omit
count_I_LSB_DL (RRC_SequenceNumber):0

#### CRLC_SetRRC_MessageSN_CNF

LLA RRC @ 00:01:18.190

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_CNF:

cellId:-1

routingInfo:

rB_Identity:2

#### CRLC_SetRRC_MessageSN_REQ

RRC LLA @ 00:01:18.190

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_REQ:

cellId:-1

routingInfo:

rB_Identity:3

count_I_LSB_UL (RRC_SequenceNumber): Omit
count_I_LSB_DL (RRC_SequenceNumber):0

#### CRLC_SetRRC_MessageSN_CNF

LLA RRC @ 00:01:18.210

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_CNF:

cellId:-1

routingInfo:

rB_Identity:3

#### CRLC_SetRRC_MessageSN_REQ

RRC LLA @ 00:01:18.210

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_REQ:

cellId:-1

routingInfo:

rB_Identity:4

count_I_LSB_UL (RRC_SequenceNumber): Omit
count_I_LSB_DL (RRC_SequenceNumber):0

#### CRLC_SetRRC_MessageSN_CNF

LLA RRC @ 00:01:18.220

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_CNF:

cellId:-1

routingInfo:

rB_Identity:4

#### CRLC_Integrity_Activate_REQ

RRC LLA @ 00:01:18.220

Cell ID: -1

Message Details:

CRLC_Integrity_Activate_REQ:

cellId:-1
cn_DomainIdentity:ps_domain

integrityActivationInfo:

integrityProtectionModeInfo:

integrityProtectionModeCommand:

startIntegrityProtection:

integrityProtInitNumber:00001111000011110000111100001111

integrityProtectionAlgorithm:uia1

#### CRLC_Integrity_Activate_REQ

RRC RLC @ 00:01:18.220

Message Details:

cellIdentity: 1

integrityActivationInfo:

integrityProtectionModeInfo:

integrityProtectionModeCommand:

startIntegrityProtection:

integrityProtInitNumber: 00001111000011110000111100001111

#### CRLC_Integrity_Activate_CNF

LLA RRC @ 00:01:18.240

Cell ID: -1

Message Details:

CRLC_Integrity_Activate_CNF:

cellId:-1

#### CRLC_Integrity_Activate_REQ

RRC LLA @ 00:01:18.240

Cell ID: -1

Message Details:

CRLC_Integrity_Activate_REQ:

cellId:-1
cn_DomainIdentity:ps_domain

integrityActivationInfo:

ul_IntegProtActivationInfo: (IntegrityProtActivationInfoList)

SS_IntegrityProtActivationTimeInfo:

rb_Identity:2
rrc_MessageSequenceNumber:0

#### CRLC_Integrity_Activate_REQ

RRC RLC @ 00:01:18.240

Message Details:

cellIdentity: 1

integrityActivationInfo:

ul_IntegrityProtActivationInfo:

rrc_MessageSequenceNumberList:

RRC_MessageSequenceNumberList.element: -2

RRC_MessageSequenceNumberList.element: -2

RRC_MessageSequenceNumberList.element: 0

RRC_MessageSequenceNumberList.element: -2

RRC_MessageSequenceNumberList.element: -2

#### CMAC Integrity Check Request

RRC MAC @ 00:01:18.250

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000001
Data:

[0]00 00 00 01
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:1 (RNC to UE)
Message Length (bits):128
Message:

[0]80 00 00 01 04 06 00 01
[8]80 01 41 E1 E1 E1 F0 18

#### CMAC Integrity Check Result

MAC RRC @ 00:01:18.250

Message Details:

Integrity Check Result:

MAC-I:00011001111101010100011100101111
Data:

[0]19 F5 47 2F

#### CRLC_Integrity_Activate_CNF

LLA RRC @ 00:01:18.250

Cell ID: -1

Message Details:

CRLC_Integrity_Activate_CNF:

cellId:-1

#### RLC_AM_DATA_REQ

RRC LLA @ 00:01:18.250

Channel ID: Rb2
Cell ID: -1

Message Details:

RLC_AM_DATA_REQ:

cellId:-1

routingInfo:

rB_Identity:2

confirmationRequest: (AmConfirmationRequest)

noConfirmationRequest:

aM_message:

dL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode:00000000000000000000000000000000
rrc_MessageSequenceNumber:0

message: (DL_DCCH_MessageType)

securityModeCommand:

r3:

securityModeCommand_r3: (SecurityModeCommand_r3_IEs)

rrc_TransactionIdentifier:0

securityCapability:

cipheringAlgorithmCap:0000000000000011
integrityProtectionAlgorithmCap:0000000000000010

cipheringModeInfo: Omit

integrityProtectionModeInfo:

integrityProtectionModeCommand:

startIntegrityProtection:

integrityProtInitNumber:00001111000011110000111100001111

integrityProtectionAlgorithm:uia1

cn_DomainIdentity:ps_domain

ue_SystemSpecificSecurityCap: (InterRAT_UE_SecurityCapList)

InterRAT_UE_SecurityCapability:

gsm:

gsmSecurityCapability:0000011

laterNonCriticalExtensions: Omit

#### RLC_AM_DATA_REQ: securityModeCommand

LLA RLC @ 00:01:18.250

Channel No: 2 Name: DCCH

Message Details:

DL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode: 00011001111101010100011100101111

rrc_MessageSequenceNumber: 1

message:

securityModeCommand:

r3:

securityModeCommand_r3:

rrc_TransactionIdentifier: 0

securityCapability:

cipheringAlgorithmCap: 0000000000000011

integrityProtectionAlgorithmCap: 0000000000000010

cipheringModeInfo: Omitted

integrityProtectionModeInfo:

integrityProtectionModeCommand:

startIntegrityProtection:

integrityProtInitNumber: 00001111000011110000111100001111

integrityProtectionAlgorithm: uia1_IntegrityProtectionAlgorithm [enum=0]

cn_DomainIdentity: ps_domain_CN_DomainIdentity [enum=1]

ue_SystemSpecificSecurityCap:

InterRAT_UE_SecurityCapList.element:

gsm:

gsmSecurityCapability: 0000011

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]8C FA A3 97 8C 06 00 01
[8]80 01 41 E1 E1 E1 F0 18

#### MAC_DATA_REQ

RLC MAC @ 00:01:18.260

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 155

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 00 8C FA A3 97 8C 06
[8]00 01 80 01 41 E1 E1 E1
[16]F0 18

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:0
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]8C FA A3 97 8C 06 00 01
[8]80 01 41 E1 E1 E1 F0 18

#### MAC_DATA_REQ

RLC MAC @ 00:01:18.260

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 155

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 0D 01 FE 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:1
Polling bit:1 (request a status report)
Length indicator 0 (octets):0 (the previous RLC PDU was exactly filled by the last segment of an RLC SDU)
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (0 octets):

Padding associated with length indicator 1 (14 octets):

[0]00 00 00 00 00 00 00 00
[8]00 00 00 00 00 00

#### PHY_DATA_REQ

MAC PHY @ 00:01:18.260

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 155

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 00 08 CF AA 39 78 C0
[8]60 00 18 00 14 1E 1E 1E
[16]1F 01 80 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 00 8C FA A3 97 8C 06
[8]00 01 80 01 41 E1 E1 E1
[16]F0 18

#### PHY_DATA_REQ

MAC PHY @ 00:01:18.270

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 156

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 00 D0 1F E0 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 0D 01 FE 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:01:18.300

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 139

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 02 50 3F E1 05 55 55
[8]55 55 55 55 55 55 55 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 25 03 FE 10 55 55 55
[8]55 55 55 55 55 55 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:01:18.300

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 139

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 25 03 FE 10 55 55 55
[8]55 55 55 55 55 55 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:4
Polling bit:1 (request a status report)
Length indicator 0 (octets):1
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (1 octets):

[0]10
Padding associated with length indicator 1 (13 octets):

[0]55 55 55 55 55 55 55 55
[8]55 55 55 55 55

#### MAC_DATA_REQ

RLC MAC @ 00:01:18.310

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 160

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 50 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:5

#### PHY_DATA_REQ

MAC PHY @ 00:01:18.310

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 160

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 05 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 50 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### MAC_DATA_REQ

RLC MAC @ 00:01:18.460

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 175

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 0D 01 FE 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:1
Polling bit:1 (request a status report)
Length indicator 0 (octets):0 (the previous RLC PDU was exactly filled by the last segment of an RLC SDU)
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (0 octets):

Padding associated with length indicator 1 (14 octets):

[0]00 00 00 00 00 00 00 00
[8]00 00 00 00 00 00

#### PHY_DATA_REQ

MAC PHY @ 00:01:18.460

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 175

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 00 D0 1F E0 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 0D 01 FE 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:01:18.500

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 159

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]10 20 02 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]02 00 20 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### MAC_DATA_IND

MAC RLC @ 00:01:18.500

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 159

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 20 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:2

#### PHY_DATA_IND

PHY MAC @ 00:01:18.510

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 160

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 01 D1 3F EC 59 1B E7
[8]10 D2 10 00 00 05 55 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 1D 13 FE C5 91 BE 71
[8]0D 21 00 00 00 55 55 55
[16]55 55

#### CMAC Integrity Check Request

RRC MAC @ 00:01:18.520

Category: Configuration

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000001
Data:

[0]00 00 00 01
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:0 (UE to RNC)
Message Length (bits):72
Message:

[0]80 00 00 01 05 21 00 00
[8]00

#### RLC_AM_DATA_IND: securityModeComplete

RLC LLA @ 00:01:18.520

Channel No: 2 Name: DCCH

Message Details:

UL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode: 10001011001000110111110011100010

rrc_MessageSequenceNumber: 1

message:

securityModeComplete:

rrc_TransactionIdentifier: 0

ul_IntegProtActivationInfo:

rrc_MessageSequenceNumberList:

RRC_MessageSequenceNumberList.element: 0

RRC_MessageSequenceNumberList.element: 0

RRC_MessageSequenceNumberList.element: 0

RRC_MessageSequenceNumberList.element: 0

RRC_MessageSequenceNumberList.element: 0

rb_UL_CiphActivationTimeInfo: Omitted

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]C5 91 BE 71 0D 21 00 00
[8]00

#### CMAC Integrity Check Result

MAC RRC @ 00:01:18.520

Message Details:

Integrity Check Result:

MAC-I:10001011001000110111110011100010
Data:

[0]8B 23 7C E2

#### MAC_DATA_IND

MAC RLC @ 00:01:18.510

BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 160

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 1D 13 FE C5 91 BE 71
[8]0D 21 00 00 00 55 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:3
Polling bit:1 (request a status report)
Length indicator 0 (octets):9
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (9 octets):

[0]C5 91 BE 71 0D 21 00 00
[8]00
Padding associated with length indicator 1 (5 octets):

[0]55 55 55 55 55

#### RLC_AM_DATA_IND

LLA RRC @ 00:01:18.520

Channel ID: Rb2
Cell ID: -1

Message Details:

RLC_AM_DATA_IND:

cellId:-1

routingInfo:

rB_Identity:2

integrityResult:

integrityUsed (IntegrityStatus):i_pass

aM_message:

uL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode:10001011001000110111110011100010
rrc_MessageSequenceNumber:1

message: (UL_DCCH_MessageType)

securityModeComplete:

rrc_TransactionIdentifier:0

ul_IntegProtActivationInfo: (IntegrityProtActivationInfo)

rrc_MessageSequenceNumberList:

RRC_MessageSequenceNumber:0
RRC_MessageSequenceNumber:0
RRC_MessageSequenceNumber:0
RRC_MessageSequenceNumber:0
RRC_MessageSequenceNumber:0

rb_UL_CiphActivationTimeInfo: (RB_ActivationTimeInfoList) Omit

laterNonCriticalExtensions: Omit

#### CRLC_Integrity_Activate_REQ

RRC LLA @ 00:01:18.520

Cell ID: -1

Message Details:

CRLC_Integrity_Activate_REQ:

cellId:-1
cn_DomainIdentity:ps_domain

integrityActivationInfo:

ul_IntegProtActivationInfo: (IntegrityProtActivationInfoList)

SS_IntegrityProtActivationTimeInfo:

rb_Identity:0
rrc_MessageSequenceNumber:0

SS_IntegrityProtActivationTimeInfo:

rb_Identity:1
rrc_MessageSequenceNumber:0

SS_IntegrityProtActivationTimeInfo:

rb_Identity:3
rrc_MessageSequenceNumber:0

SS_IntegrityProtActivationTimeInfo:

rb_Identity:4
rrc_MessageSequenceNumber:0

#### CRLC_Integrity_Activate_REQ

RRC RLC @ 00:01:18.520

Message Details:

cellIdentity: 1

integrityActivationInfo:

ul_IntegrityProtActivationInfo:

rrc_MessageSequenceNumberList:

RRC_MessageSequenceNumberList.element: 0

RRC_MessageSequenceNumberList.element: 0

RRC_MessageSequenceNumberList.element: -2

RRC_MessageSequenceNumberList.element: 0

RRC_MessageSequenceNumberList.element: 0

#### MAC_DATA_REQ

RLC MAC @ 00:01:18.520

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 181

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 40 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:4

#### PHY_DATA_REQ

MAC PHY @ 00:01:18.520

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 181

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]10 20 04 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]02 00 40 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### CMAC Integrity Check Request

RRC MAC @ 00:01:18.540

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000001
Data:

[0]00 00 00 01
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:1 (RNC to UE)
Message Length (bits):240
Message:

[0]80 00 00 01 81 42 02 A1
[8]00 40 64 C0 80 1E 22 00
[16]00 20 A3 35 62 46 E3 00
[24]BE 81 30 EC A8 60

#### CMAC Integrity Check Result

MAC RRC @ 00:01:18.540

Message Details:

Integrity Check Result:

MAC-I:01010011010110111100110000111101
Data:

[0]53 5B CC 3D

#### CRLC_Integrity_Activate_CNF

LLA RRC @ 00:01:18.540

Cell ID: -1

Message Details:

CRLC_Integrity_Activate_CNF:

cellId:-1

#### RRC_DATA_REQ: gmm:attachAccept

NAS RRC @ 00:01:18.540

Cell ID: -1

Message Details:

ATTACHACCEPT:

skipIndicator: 0000

gMMProtocolDiscriminator: 1000

msgType: 00000010

forceToStandby:

spare: 0

value: 000

attachResult:

spare: 0

result: 011

periodicRAupdateTimer:

unit: 001

value: 00110

spare: 0000

radioPrioSMS:

spare: 0

value: 100

rai:

plmn: 00F110

lac: 0001

rac: 05

ptmsiSignature:

iei: 00011001

value: AB1237

negReadyTimer: Omitted

allocatedPTMSI:

iei: 00011000

iel: 05

iDigit1: 1111

oddEvenInd: 0

typeOfId: 100

otherDigits: 09876543

msIdentity: Omitted

gmmCause: Omitted

t3302Value: Omitted

cellNotification: Omitted

equivalentPLMN: Omitted

#### RLC_AM_DATA_REQ:downlinkDirectTransfer

RRC RLC @ 00:01:18.540

Channel No: 3 Name: DCCH

Message Details:

Opt1: 0

Opt2: 0

DL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode: 01010011010110111100110000111101

rrc_MessageSequenceNumber: 1

message:

downlinkDirectTransfer:

r3:

downlinkDirectTransfer_r3:

rrc_TransactionIdentifier: 0

cn_DomainIdentity: ps_domain_CN_DomainIdentity [enum=1]

nas_Message: 080203260400F11000010519AB12371805F409876543

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]A9 AD E6 1E 89 42 02 A1
[8]00 40 64 C0 80 1E 22 00
[16]00 20 A3 35 62 46 E3 00
[24]BE 81 30 EC A8 60

#### MAC_DATA_REQ

RLC MAC @ 00:01:18.550

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 184

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 18 A9 AD E6 1E 89 42
[8]02 A1 00 40 64 C0 80 1E
[16]22 00

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:3
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]A9 AD E6 1E 89 42 02 A1
[8]00 40 64 C0 80 1E 22 00

#### MAC_DATA_REQ

RLC MAC @ 00:01:18.550

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 184

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 25 1D FE 00 20 A3 35
[8]62 46 E3 00 BE 81 30 EC
[16]A8 60

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:4
Polling bit:1 (request a status report)
Length indicator 0 (octets):14
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (14 octets):

[0]00 20 A3 35 62 46 E3 00
[8]BE 81 30 EC A8 60
Padding associated with length indicator 1 (0 octets):

#### PHY_DATA_REQ

MAC PHY @ 00:01:18.550

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 184

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 01 8A 9A DE 61 E8 94
[8]20 2A 10 04 06 4C 08 01
[16]E2 20 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 18 A9 AD E6 1E 89 42
[8]02 A1 00 40 64 C0 80 1E
[16]22 00

#### PHY_DATA_REQ

MAC PHY @ 00:01:18.560

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 185

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 02 51 DF E0 02 0A 33
[8]56 24 6E 30 0B E8 13 0E
[16]CA 86 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 25 1D FE 00 20 A3 35
[8]62 46 E3 00 BE 81 30 EC
[16]A8 60

#### PHY_DATA_IND

PHY MAC @ 00:01:18.710

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 180

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]10 20 02 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]02 00 20 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### MAC_DATA_IND

MAC RLC @ 00:01:18.710

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 180

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 20 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:2

#### PHY_DATA_IND

PHY MAC @ 00:01:18.720

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 181

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 01 D1 3F EC 59 1B E7
[8]10 D2 10 00 00 05 55 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 1D 13 FE C5 91 BE 71
[8]0D 21 00 00 00 55 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:01:18.720

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 181

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 1D 13 FE C5 91 BE 71
[8]0D 21 00 00 00 55 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:3
Polling bit:1 (request a status report)
Length indicator 0 (octets):9
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (9 octets):

[0]C5 91 BE 71 0D 21 00 00
[8]00
Padding associated with length indicator 1 (5 octets):

[0]55 55 55 55 55

#### MAC_DATA_REQ

RLC MAC @ 00:01:18.730

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 202

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 40 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:4

#### PHY_DATA_REQ

MAC PHY @ 00:01:18.730

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 202

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]10 20 04 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]02 00 40 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### MAC_DATA_REQ

RLC MAC @ 00:01:18.750

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 204

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 25 1D FE 00 20 A3 35
[8]62 46 E3 00 BE 81 30 EC
[16]A8 60

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:4
Polling bit:1 (request a status report)
Length indicator 0 (octets):14
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (14 octets):

[0]00 20 A3 35 62 46 E3 00
[8]BE 81 30 EC A8 60
Padding associated with length indicator 1 (0 octets):

#### PHY_DATA_REQ

MAC PHY @ 00:01:18.750

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 204

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 02 51 DF E0 02 0A 33
[8]56 24 6E 30 0B E8 13 0E
[16]CA 86 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 25 1D FE 00 20 A3 35
[8]62 46 E3 00 BE 81 30 EC
[16]A8 60

#### PHY_DATA_IND

PHY MAC @ 00:01:18.790

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 188

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 05 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 50 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### MAC_DATA_IND

MAC RLC @ 00:01:18.790

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 188

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 50 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:5

#### PHY_DATA_IND

PHY MAC @ 00:01:18.800

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 189

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 02 D1 5F ED 6F 6F 71
[8]E0 EC 80 08 40 18 05 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 2D 15 FE D6 F6 F7 1E
[8]0E C8 00 84 01 80 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:01:18.800

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 189

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 2D 15 FE D6 F6 F7 1E
[8]0E C8 00 84 01 80 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:5
Polling bit:1 (request a status report)
Length indicator 0 (octets):10
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (10 octets):

[0]D6 F6 F7 1E 0E C8 00 84
[8]01 80
Padding associated with length indicator 1 (4 octets):

[0]55 55 55 55

#### RLC_AM_DATA_IND: uplinkDirectTransfer

RLC RRC @ 00:01:18.810

Channel No: 3 Name: DCCH

Message Details:

UL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode: 10101101111011011110111000111100

rrc_MessageSequenceNumber: 1

message:

uplinkDirectTransfer:

cn_DomainIdentity: ps_domain_CN_DomainIdentity [enum=1]

nas_Message: 0803

measuredResultsOnRACH: Omitted

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]D6 F6 F7 1E 0E C8 00 84
[8]01 80

#### RRC_DATA_IND: gmm:attachComplete

RRC NAS @ 00:01:18.810

Cell ID: -1

Message Details:

ATTACHCOMPLETE:

skipIndicator: 0000

gMMProtocolDiscriminator: 1000

msgType: 00000011

#### MAC_DATA_REQ

RLC MAC @ 00:01:18.810

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 210

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 60 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:6

#### PHY_DATA_REQ

MAC PHY @ 00:01:18.810

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 210

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 06 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 60 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### CMAC Integrity Check Request

RRC MAC @ 00:01:18.830

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000001
Data:

[0]00 00 00 01
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:0 (UE to RNC)
Message Length (bits):80
Message:

[0]80 00 00 01 86 C8 00 84
[8]01 80

#### CMAC Integrity Check Result

MAC RRC @ 00:01:18.830

Message Details:

Integrity Check Result:

MAC-I:10101101111011011110111000111100
Data:

[0]AD ED EE 3C

#### PHY_DATA_IND

PHY MAC @ 00:01:19.000

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 209

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 05 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 50 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### MAC_DATA_IND

MAC RLC @ 00:01:19.000

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 209

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 50 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:5

#### PHY_DATA_IND

PHY MAC @ 00:01:19.010

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 210

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 02 D1 5F ED 6F 6F 71
[8]E0 EC 80 08 40 18 05 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 2D 15 FE D6 F6 F7 1E
[8]0E C8 00 84 01 80 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:01:19.010

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 210

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 2D 15 FE D6 F6 F7 1E
[8]0E C8 00 84 01 80 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:5
Polling bit:1 (request a status report)
Length indicator 0 (octets):10
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (10 octets):

[0]D6 F6 F7 1E 0E C8 00 84
[8]01 80
Padding associated with length indicator 1 (4 octets):

[0]55 55 55 55

#### MAC_DATA_REQ

RLC MAC @ 00:01:19.020

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 231

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 60 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:6

#### PHY_DATA_REQ

MAC PHY @ 00:01:19.020

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 231

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 06 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 60 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### CMAC Integrity Check Request

RRC MAC @ 00:01:19.830

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000001
Data:

[0]00 00 00 01
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:1 (RNC to UE)
Message Length (bits):56
Message:

[0]80 00 00 00 83 C8 00

#### CMAC Integrity Check Result

MAC RRC @ 00:01:19.830

Message Details:

Integrity Check Result:

MAC-I:11101100100111000001011111010011
Data:

[0]EC 9C 17 D3

#### RLC_UM_DATA_REQ

RRC LLA @ 00:01:19.830

Channel ID: Rb1
Cell ID: -1

Message Details:

RLC_UM_DATA_REQ:

cellId:-1

routingInfo:

rB_Identity:1

uM_message:

dL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode:00000000000000000000000000000000
rrc_MessageSequenceNumber:0

message: (DL_DCCH_MessageType)

rrcConnectionRelease:

r3:

rrcConnectionRelease_r3: (RRCConnectionRelease_r3_IEs)

rrc_TransactionIdentifier:0
n_308:1
releaseCause:normalEvent

rplmn_information: Omit

laterNonCriticalExtensions: Omit

specialLI:false

#### RLC_UM_DATA_REQ: rrcConnectionRelease

LLA RLC @ 00:01:19.830

Channel No: 1 Name: DCCH

Message Details:

DL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode: 11101100100111000001011111010011

rrc_MessageSequenceNumber: 1

message:

rrcConnectionRelease:

r3:

rrcConnectionRelease_r3:

rrc_TransactionIdentifier: 0

n_308: 1

releaseCause: normalEvent_ReleaseCause [enum=0]

rplmn_information: Omitted

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]F6 4E 0B E9 8B C8 00

#### MAC_DATA_REQ

RLC MAC @ 00:01:19.840

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 57

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]01 0F FE F6 4E 0B E9 8B
[8]C8 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

Sequence number:0
Length indicator 0 (octets):7
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (7 octets):

[0]F6 4E 0B E9 8B C8 00
Padding associated with length indicator 1 (8 octets):

[0]00 00 00 00 00 00 00 00

#### PHY_DATA_REQ

MAC PHY @ 00:01:19.840

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 57

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]00 10 FF EF 64 E0 BE 98
[8]BC 80 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:0
MAC SDU (144 bits):

[0]01 0F FE F6 4E 0B E9 8B
[8]C8 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:01:20.080

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 61

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]00 10 DF EF BF 16 16 70
[8]C4 05 55 55 55 55 55 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:0
MAC SDU (144 bits):

[0]01 0D FE FB F1 61 67 0C
[8]40 55 55 55 55 55 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:01:20.080

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 61

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]01 0D FE FB F1 61 67 0C
[8]40 55 55 55 55 55 55 55
[16]55 55

RLC PDU (decoded):

Sequence number:0
Length indicator 0 (octets):6
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (6 octets):

[0]FB F1 61 67 0C 40
Padding associated with length indicator 1 (9 octets):

[0]55 55 55 55 55 55 55 55
[8]55

#### CMAC Integrity Check Request

RRC MAC @ 00:01:20.100

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000001
Data:

[0]00 00 00 01
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:0 (UE to RNC)
Message Length (bits):48
Message:

[0]80 00 00 00 84 40

#### RLC_UM_DATA_IND: rrcConnectionReleaseComplete

RLC LLA @ 00:01:20.100

Channel No: 1 Name: DCCH

Message Details:

UL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode: 11110111111000101100001011001110

rrc_MessageSequenceNumber: 1

message:

rrcConnectionReleaseComplete:

rrc_TransactionIdentifier: 0

errorIndication: Omitted

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]FB F1 61 67 0C 40

#### CMAC Integrity Check Result

MAC RRC @ 00:01:20.100

Message Details:

Integrity Check Result:

MAC-I:11110111111000101100001011001110
Data:

[0]F7 E2 C2 CE

#### RLC_UM_DATA_IND

LLA RRC @ 00:01:20.100

Channel ID: Rb1
Cell ID: -1

Message Details:

RLC_UM_DATA_IND:

cellId:-1

routingInfo:

rB_Identity:1

integrityResult:

integrityUsed (IntegrityStatus):i_pass

uM_message:

uL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode:11110111111000101100001011001110
rrc_MessageSequenceNumber:1

message: (UL_DCCH_MessageType)

rrcConnectionReleaseComplete:

rrc_TransactionIdentifier:0

errorIndication: (FailureCauseWithProtErr) Omit

laterNonCriticalExtensions: Omit

#### PHY_DATA_IND

PHY MAC @ 00:01:20.240

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 77

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]00 30 DF ED CD 18 3E 01
[8]44 05 55 55 55 55 55 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:0
MAC SDU (144 bits):

[0]03 0D FE DC D1 83 E0 14
[8]40 55 55 55 55 55 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:01:20.240

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 77

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]03 0D FE DC D1 83 E0 14
[8]40 55 55 55 55 55 55 55
[16]55 55

RLC PDU (decoded):

Sequence number:1
Length indicator 0 (octets):6
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (6 octets):

[0]DC D1 83 E0 14 40
Padding associated with length indicator 1 (9 octets):

[0]55 55 55 55 55 55 55 55
[8]55

#### CPHY_OUTSYNC_IND

PHY RRC @ 00:01:20.300

BTS unit: 1:1
Channel No: 0 Name: U_DPCH
CFN: 103

Message Details:

#### CMAC Integrity Check Request

RRC MAC @ 00:01:20.330

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000010
Data:

[0]00 00 00 02
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:0 (UE to RNC)
Message Length (bits):48
Message:

[0]80 00 00 00 84 40

#### RLC_UM_DATA_IND: rrcConnectionReleaseComplete

RLC LLA @ 00:01:20.330

Channel No: 1 Name: DCCH

Message Details:

UL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode: 10111001101000110000011111000000

rrc_MessageSequenceNumber: 2

message:

rrcConnectionReleaseComplete:

rrc_TransactionIdentifier: 0

errorIndication: Omitted

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]DC D1 83 E0 14 40

#### CMAC Integrity Check Result

MAC RRC @ 00:01:20.330

Message Details:

Integrity Check Result:

MAC-I:10111001101000110000011111000000
Data:

[0]B9 A3 07 C0

#### RLC_UM_DATA_IND

LLA RRC @ 00:01:20.330

Channel ID: Rb1
Cell ID: -1

Message Details:

RLC_UM_DATA_IND:

cellId:-1

routingInfo:

rB_Identity:1

integrityResult:

integrityUsed (IntegrityStatus):i_pass

uM_message:

uL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode:10111001101000110000011111000000
rrc_MessageSequenceNumber:2

message: (UL_DCCH_MessageType)

rrcConnectionReleaseComplete:

rrc_TransactionIdentifier:0

errorIndication: (FailureCauseWithProtErr) Omit

laterNonCriticalExtensions: Omit

#### CRLC_Config_REQ

RRC LLA @ 00:01:20.330

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:1

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC UM Channel Release REQ

LLA RLC @ 00:01:20.340

BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 107

Message Details:

#### CRLC UM Channel Release CNF

RLC LLA @ 00:01:20.340

BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 107

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:01:20.350

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:1

#### CRLC_Config_REQ

RRC LLA @ 00:01:20.350

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:2

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC AM Channel Release REQ

LLA RLC @ 00:01:20.350

BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 108

Message Details:

#### CRLC AM Channel Release CNF

RLC LLA @ 00:01:20.350

BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 108

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:01:20.360

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:2

#### CRLC_Config_REQ

RRC LLA @ 00:01:20.360

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:3

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC AM Channel Release REQ

LLA RLC @ 00:01:20.370

BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 110

Message Details:

#### CRLC AM Channel Release CNF

RLC LLA @ 00:01:20.370

BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 110

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:01:20.380

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:3

#### CRLC_Config_REQ

RRC LLA @ 00:01:20.380

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:4

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC AM Channel Release REQ

LLA RLC @ 00:01:20.380

BTS unit: 1:1
Channel No: 4 Name: DCCH
CFN: 111

Message Details:

#### CRLC AM Channel Release CNF

RLC LLA @ 00:01:20.380

BTS unit: 1:1
Channel No: 4 Name: DCCH
CFN: 111

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:01:20.390

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:4

#### CRLC_Config_REQ

RRC LLA @ 00:01:20.390

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:1

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode)

dl_UM_RLC_Mode:

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):136

dl_RLCModeInfo: (UL_RLC_Mode)

ul_UM_RLC_Mode:

transmissionRLC_Discard:

timerBasedNoExplicit (NoExplicitDiscard):dt100

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity):1
dLlogicalChannelIdentity (LogicalChannelIdentity):1
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC UM Channel Establish REQ

LLA RLC @ 00:01:20.400

BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 113

Message Details:

Configuration Parameters:

PU Size In Bits:136

#### CRLC UM Channel Establish CNF

RLC LLA @ 00:01:20.400

BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 113

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:01:20.410

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:1

#### CRLC_Config_REQ

RRC LLA @ 00:01:20.410

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:2

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode)

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):128

dl_RLCModeInfo: (UL_RLC_Mode)

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity):2
dLlogicalChannelIdentity (LogicalChannelIdentity):2
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC AM Channel Establish REQ

LLA RLC @ 00:01:20.410

BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 114

Message Details:

Configuration Parameters:

PU Size In Bits:128

Timer Parameters:

Poll (ms):200
Poll Prohibit (ms):0
EPC (ms):0
Discard (ms):0
Poll Periodic (ms):0
Status Prohibit (ms):0
Status Periodic (ms):0
Reset (ms):500
MRW (ms):0

Protocol Parameters:

Max Dat:15
Poll PU:0
Poll SDU:1
Poll Window:99
Max Reset:1
Tx Window Size:32
Rx Window Size:32
Max MRW:0
SDU Discard Mode:No discard

Polling Triggers:

Last PU In Buffer:On
Last PU In Retransmission Buffer:On
Poll Timer:On
Every Poll-PU PU:Off
Every Poll-SDU SDU:On
Poll-Window Percent Of Transmission Buffer:On
Timer Based:Off

Status Triggers:

Missing PU:On
Timer Based:Off
EPC Mechanism:Off

#### CRLC AM Channel Establish CNF

RLC LLA @ 00:01:20.410

BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 114

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:01:20.430

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:2

#### CRLC_Config_REQ

RRC LLA @ 00:01:20.430

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:3

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode)

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):128

dl_RLCModeInfo: (UL_RLC_Mode)

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity):3
dLlogicalChannelIdentity (LogicalChannelIdentity):3
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC AM Channel Establish REQ

LLA RLC @ 00:01:20.430

BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 116

Message Details:

Configuration Parameters:

PU Size In Bits:128

Timer Parameters:

Poll (ms):200
Poll Prohibit (ms):0
EPC (ms):0
Discard (ms):0
Poll Periodic (ms):0
Status Prohibit (ms):0
Status Periodic (ms):0
Reset (ms):500
MRW (ms):0

Protocol Parameters:

Max Dat:15
Poll PU:0
Poll SDU:1
Poll Window:99
Max Reset:1
Tx Window Size:32
Rx Window Size:32
Max MRW:0
SDU Discard Mode:No discard

Polling Triggers:

Last PU In Buffer:On
Last PU In Retransmission Buffer:On
Poll Timer:On
Every Poll-PU PU:Off
Every Poll-SDU SDU:On
Poll-Window Percent Of Transmission Buffer:On
Timer Based:Off

Status Triggers:

Missing PU:On
Timer Based:Off
EPC Mechanism:Off

#### CRLC AM Channel Establish CNF

RLC LLA @ 00:01:20.430

BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 116

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:01:20.440

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:3

#### CRLC_Config_REQ

RRC LLA @ 00:01:20.440

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:4

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode)

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):128

dl_RLCModeInfo: (UL_RLC_Mode)

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity):4
dLlogicalChannelIdentity (LogicalChannelIdentity):4
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC AM Channel Establish REQ

LLA RLC @ 00:01:20.450

BTS unit: 1:1
Channel No: 4 Name: DCCH
CFN: 118

Message Details:

Configuration Parameters:

PU Size In Bits:128

Timer Parameters:

Poll (ms):200
Poll Prohibit (ms):0
EPC (ms):0
Discard (ms):0
Poll Periodic (ms):0
Status Prohibit (ms):0
Status Periodic (ms):0
Reset (ms):500
MRW (ms):0

Protocol Parameters:

Max Dat:15
Poll PU:0
Poll SDU:1
Poll Window:99
Max Reset:1
Tx Window Size:32
Rx Window Size:32
Max MRW:0
SDU Discard Mode:No discard

Polling Triggers:

Last PU In Buffer:On
Last PU In Retransmission Buffer:On
Poll Timer:On
Every Poll-PU PU:Off
Every Poll-SDU SDU:On
Poll-Window Percent Of Transmission Buffer:On
Timer Based:Off

Status Triggers:

Missing PU:On
Timer Based:Off
EPC Mechanism:Off

#### CRLC AM Channel Establish CNF

RLC LLA @ 00:01:20.450

BTS unit: 1:1
Channel No: 4 Name: DCCH
CFN: 118

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:01:20.460

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:4

#### PHY_DATA_IND

PHY MAC @ 00:07:20.580

BTS unit: 1:1
Channel No: 0 Name: U_RACH
CFN: 15

Message Details:

TFI:0
TB set size:168
TB size:168
TB set (raw):

[0]08 44 48 8C D1 00 04 02
[8]00 02 C0 00 00 00 00 00
[16]00 00 00 00 00 00

TB set (decoded):

TB 0:

TCTF:0
MAC SDU (166 bits):

[0]21 11 22 33 44 00 10 08
[8]00 0B 00 00 00 00 00 00
[16]00 00 00 00 00

#### MAC_DATA_IND

MAC RLC @ 00:07:20.580

Category: Configuration
BTS unit: 1:1
Channel No: 0 Name: CCCH
CFN: 15

Message Details:

RLC PDU size (bits):166
RLC PDU (raw):

[0]21 11 22 33 44 00 10 08
[8]00 0B 00 00 00 00 00 00
[16]00 00 00 00 00

#### RLC_TR_DATA_IND: rrcConnectionRequest

RLC LLA @ 00:07:20.630

Channel No: 0 Name: CCCH

Message Details:

UL_CCCH_Message:

integrityCheckInfo: Omitted

message:

rrcConnectionRequest:

initialUE_Identity:

tmsi_and_LAI:

tmsi: 00010001001000100011001101000100

lai:

plmn_Identity:

mcc:

MCC.element: 0

MCC.element: 0

MCC.element: 1

mnc:

MNC.element: 0

MNC.element: 1

lac: 0000000000000001

establishmentCause: registration_EstablishmentCause [enum=12]

protocolErrorIndicator: noError_ProtocolErrorIndicator [enum=0]

measuredResultsOnRACH: Omitted

v3d0NonCriticalExtensions: Omitted

Layer 3 SDU:

[0]21 11 22 33 44 00 10 08
[8]00 0B 00 00 00 00 00 00
[16]00 00 00 00 00

#### RLC_TR_DATA_IND

LLA RRC @ 00:07:20.630

Channel ID: Rb0
Cell ID: 0

Message Details:

RLC_TR_DATA_IND:

cellId:0

routingInfo:

rB_Identity:0

tM_message:

uL_CCCH_Message:

integrityCheckInfo: Omit

message: (UL_CCCH_MessageType)

rrcConnectionRequest:

initialUE_Identity:

tmsi_and_LAI: (TMSI_and_LAI_GSM_MAP)

tmsi (TMSI_GSM_MAP):00010001001000100011001101000100

lai:

plmn_Identity:

mcc:

Digit:0
Digit:0
Digit:1

mnc:

Digit:0
Digit:1

lac:0000000000000001

establishmentCause:registration
protocolErrorIndicator:noError

measuredResultsOnRACH: Omit

v3d0NonCriticalExtensions: Omit

#### RLC_UM_DATA_REQ

RRC LLA @ 00:07:20.630

Channel ID: Rb0
Cell ID: 0

Message Details:

RLC_UM_DATA_REQ:

cellId:0

routingInfo:

rB_Identity:0

uM_message:

dL_CCCH_Message:

integrityCheckInfo: Omit

message: (DL_CCCH_MessageType)

rrcConnectionSetup:

r3:

rrcConnectionSetup_r3: (RRCConnectionSetup_r3_IEs)

initialUE_Identity:

tmsi_and_LAI: (TMSI_and_LAI_GSM_MAP)

tmsi (TMSI_GSM_MAP):00010001001000100011001101000100

lai:

plmn_Identity:

mcc:

Digit:0
Digit:0
Digit:1

mnc:

Digit:0
Digit:1

lac:0000000000000001

rrc_TransactionIdentifier:0
activationTime: Omit

new_U_RNTI: (U_RNTI)

srnc_Identity:000000000001
s_RNTI:00000000000000000001

new_c_RNTI (C_RNTI): Omit
rrc_StateIndicator:cell_DCH
utran_DRX_CycleLengthCoeff (UTRAN_DRX_CycleLengthCoefficient):9

capabilityUpdateRequirement:

ue_RadioCapabilityFDDUpdateRequirement:true
ue_RadioCapabilityTDDUpdateRequirement:false

systemSpecificCapUpdateReqList:

SystemSpecificCapUpdateReq:gsm

srb_InformationSetupList: (SRB_InformationSetupList2)

SRB_InformationSetup:

rb_Identity: Omit

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_UM_RLC_Mode:

transmissionRLC_Discard: Omit

dl_RLC_Mode:

dl_UM_RLC_Mode:

rb_MappingInfo:

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

dch (TransportChannelIdentity):5

logicalChannelIdentity:1

rlc_SizeList:

configured:

mac_LogicalChannelPriority:1

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

dch (TransportChannelIdentity):10

logicalChannelIdentity:1

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

rach:

logicalChannelIdentity:1

rlc_SizeList:

explicitList: (RLC_SizeExplicitList)

RLC_SizeInfo:

rlc_SizeIndex:1

mac_LogicalChannelPriority:1

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

fach:

logicalChannelIdentity:1

SRB_InformationSetup:

rb_Identity: Omit

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

rb_MappingInfo:

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

dch (TransportChannelIdentity):5

logicalChannelIdentity:2

rlc_SizeList:

configured:

mac_LogicalChannelPriority:2

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

dch (TransportChannelIdentity):10

logicalChannelIdentity:2

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

rach:

logicalChannelIdentity:2

rlc_SizeList:

explicitList: (RLC_SizeExplicitList)

RLC_SizeInfo:

rlc_SizeIndex:1

mac_LogicalChannelPriority:2

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

fach:

logicalChannelIdentity:2

SRB_InformationSetup:

rb_Identity: Omit

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

rb_MappingInfo:

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

dch (TransportChannelIdentity):5

logicalChannelIdentity:3

rlc_SizeList:

configured:

mac_LogicalChannelPriority:3

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

dch (TransportChannelIdentity):10

logicalChannelIdentity:3

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

rach:

logicalChannelIdentity:3

rlc_SizeList:

explicitList: (RLC_SizeExplicitList)

RLC_SizeInfo:

rlc_SizeIndex:1

mac_LogicalChannelPriority:3

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

fach:

logicalChannelIdentity:3

SRB_InformationSetup:

rb_Identity: Omit

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

rb_MappingInfo:

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

dch (TransportChannelIdentity):5

logicalChannelIdentity:4

rlc_SizeList:

configured:

mac_LogicalChannelPriority:4

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

dch (TransportChannelIdentity):10

logicalChannelIdentity:4

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

rach:

logicalChannelIdentity:4

rlc_SizeList:

explicitList: (RLC_SizeExplicitList)

RLC_SizeInfo:

rlc_SizeIndex:1

mac_LogicalChannelPriority:4

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

fach:

logicalChannelIdentity:4

ul_CommonTransChInfo:

tfc_Subset: Omit

prach_TFCS: (TFCS) Omit

modeSpecificInfo:

fdd:

ul_TFCS: (TFCS)

normalTFCI_Signalling: (ExplicitTFCS_Configuration)

complete: (TFCS_ReconfAdd)

ctfcSize:

ctfc2Bit:

:

ctfc2:0

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc2:1

powerOffsetInformation:

gainFactorInformation:

signalledGainFactors:

modeSpecificInfo:

fdd:

gainFactorBetaC (GainFactor):11

gainFactorBetaD (GainFactor):15
referenceTFC_ID:0

powerOffsetPp_m: Omit

ul_AddReconfTransChInfoList:

UL_AddReconfTransChInformation:

ul_TransportChannelType (UL_TrCH_Type):dch
transportChannelIdentity:5

transportFormatSet:

dedicatedTransChTFS:

tti:

tti10: (DedicatedDynamicTF_InfoList)

DedicatedDynamicTF_Info:

rlc_Size:

bitMode: (BitModeRLC_SizeInfo)

sizeType2:

part1:2
part2: Omit

numberOfTbSizeList:

NumberOfTransportBlocks:

zero:

NumberOfTransportBlocks:

one:

logicalChannelList:

allSizes:

semistaticTF_Information:

channelCodingType:

convolutional (CodingRate):third

rateMatchingAttribute:192
crc_Size:crc16

dl_CommonTransChInfo:

sccpch_TFCS: (TFCS) Omit

modeSpecificInfo:

fdd:

dl_Parameters:

sameAsUL:

dl_AddReconfTransChInfoList:

DL_AddReconfTransChInformation:

dl_TransportChannelType (DL_TrCH_Type):dch
dl_transportChannelIdentity (TransportChannelIdentity):10

tfs_SignallingMode:

sameAsULTrCH: (UL_TransportChannelIdentity)

ul_TransportChannelType (UL_TrCH_Type):dch
ul_TransportChannelIdentity (TransportChannelIdentity):5

dch_QualityTarget: (QualityTarget)

bler_QualityValue:-20

dummy: (TM_SignallingInfo) Omit

frequencyInfo: Omit

maxAllowedUL_TX_Power: Omit

ul_ChannelRequirement:

ul_DPCH_Info:

ul_DPCH_PowerControlInfo:

fdd:

dpcch_PowerOffset:-40
pc_Preamble:1
sRB_delay:7

powerControlAlgorithm:

algorithm1 (TPC_StepSizeFDD):0

modeSpecificInfo:

fdd:

scramblingCodeType:longSC
scramblingCode (UL_ScramblingCode):0
numberOfDPDCH: Omit
spreadingFactor:sf64
tfci_Existence:true
numberOfFBI_Bits: Omit
puncturingLimit:pl1

dl_CommonInformation:

dl_DPCH_InfoCommon:

cfnHandling:

initialise:

cfntargetsfnframeoffset: Omit

modeSpecificInfo:

fdd:

dl_DPCH_PowerControlInfo:

modeSpecificInfo:

fdd:

dpc_Mode:singleTPC

powerOffsetPilot_pdpdch:0

dl_rate_matching_restriction: Omit

spreadingFactorAndPilot: (SF512_AndPilot)

sfd128 (PilotBits128):pb4

positionFixedOrFlexible:fixed
tfci_Existence:false

modeSpecificInfo:

fdd:

defaultDPCH_OffsetValue (DefaultDPCH_OffsetValueFDD):0

dpch_CompressedModeInfo: Omit

tx_DiversityMode:noDiversity

ssdt_Information: Omit

dl_InformationPerRL_List:

DL_InformationPerRL:

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode:100

pdsch_SHO_DCH_Info: Omit

pdsch_CodeMapping: Omit

dl_DPCH_InfoPerRL:

fdd:

pCPICH_UsageForChannelEst:mayBeUsed
dpch_FrameOffset:0

secondaryCPICH_Info: Omit

dl_ChannelisationCodeList:

DL_ChannelisationCode:

secondaryScramblingCode:1

sf_AndCodeNumber: (SF512_AndCodeNumber)

sf128:0

scramblingCodeChange:noCodeChange

tpc_CombinationIndex:0
ssdt_CellIdentity: Omit
closedLoopTimingAdjMode: Omit

sccpch_InfoforFACH: Omit

laterNonCriticalExtensions: Omit

specialLI:true

#### RLC_UM_DATA_REQ: rrcConnectionSetup

LLA RLC @ 00:07:20.630

Channel No: 1 Name: CCCH

Message Details:

DL_CCCH_Message:

integrityCheckInfo: Omitted

message:

rrcConnectionSetup:

r3:

rrcConnectionSetup_r3:

initialUE_Identity:

tmsi_and_LAI:

tmsi: 00010001001000100011001101000100

lai:

plmn_Identity:

mcc:

MCC.element: 0

MCC.element: 0

MCC.element: 1

mnc:

MNC.element: 0

MNC.element: 1

lac: 0000000000000001

rrc_TransactionIdentifier: 0

activationTime: Omitted

new_U_RNTI:

srnc_Identity: 000000000001

s_RNTI: 00000000000000000001

new_c_RNTI: Omitted

rrc_StateIndicator: cell_DCH_RRC_StateIndicator [enum=0]

utran_DRX_CycleLengthCoeff: 9

capabilityUpdateRequirement:

ue_RadioCapabilityFDDUpdateRequirement: 1

ue_RadioCapabilityTDDUpdateRequirement: 0

systemSpecificCapUpdateReqList:

SystemSpecificCapUpdateReqList.element: gsm_SystemSpecificCapUpdateReq [enum=0]

srb_InformationSetupList:

SRB_InformationSetupList2.element:

rb_Identity: Omitted

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_UM_RLC_Mode:

transmissionRLC_Discard: Omitted

dl_RLC_Mode:

dl_UM_RLC_Mode: NULL

rb_MappingInfo:

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

dch: 5

logicalChannelIdentity: 1

rlc_SizeList:

configured: NULL

mac_LogicalChannelPriority: 1

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

dch: 10

logicalChannelIdentity: 1

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

rach: NULL

logicalChannelIdentity: 1

rlc_SizeList:

explicitList:

RLC_SizeExplicitList.element:

rlc_SizeIndex: 1

mac_LogicalChannelPriority: 1

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

fach: NULL

logicalChannelIdentity: 1

SRB_InformationSetupList2.element:

rb_Identity: Omitted

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard: dat15_MaxDAT [enum=10]

transmissionWindowSize: tw32_TransmissionWindowSize [enum=3]

timerRST: tr500_TimerRST [enum=9]

max_RST: rst1_MaxRST [enum=0]

pollingInfo:

timerPollProhibit: tpp200_TimerPollProhibit [enum=19]

timerPoll: tp200_TimerPoll [enum=19]

poll_PDU: Omitted

poll_SDU: sdu1_Poll_SDU [enum=0]

lastTransmissionPDU_Poll: 1

lastRetransmissionPDU_Poll: 1

pollWindow: pw99_PollWindow [enum=7]

timerPollPeriodic: Omitted

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery: 1

receivingWindowSize: rw32_ReceivingWindowSize [enum=3]

dl_RLC_StatusInfo:

timerStatusProhibit: tsp200_TimerStatusProhibit [enum=19]

timerEPC: Omitted

missingPDU_Indicator: 1

timerStatusPeriodic: Omitted

rb_MappingInfo:

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

dch: 5

logicalChannelIdentity: 2

rlc_SizeList:

configured: NULL

mac_LogicalChannelPriority: 2

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

dch: 10

logicalChannelIdentity: 2

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

rach: NULL

logicalChannelIdentity: 2

rlc_SizeList:

explicitList:

RLC_SizeExplicitList.element:

rlc_SizeIndex: 1

mac_LogicalChannelPriority: 2

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

fach: NULL

logicalChannelIdentity: 2

SRB_InformationSetupList2.element:

rb_Identity: Omitted

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard: dat15_MaxDAT [enum=10]

transmissionWindowSize: tw32_TransmissionWindowSize [enum=3]

timerRST: tr500_TimerRST [enum=9]

max_RST: rst1_MaxRST [enum=0]

pollingInfo:

timerPollProhibit: tpp200_TimerPollProhibit [enum=19]

timerPoll: tp200_TimerPoll [enum=19]

poll_PDU: Omitted

poll_SDU: sdu1_Poll_SDU [enum=0]

lastTransmissionPDU_Poll: 1

lastRetransmissionPDU_Poll: 1

pollWindow: pw99_PollWindow [enum=7]

timerPollPeriodic: Omitted

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery: 1

receivingWindowSize: rw32_ReceivingWindowSize [enum=3]

dl_RLC_StatusInfo:

timerStatusProhibit: tsp200_TimerStatusProhibit [enum=19]

timerEPC: Omitted

missingPDU_Indicator: 1

timerStatusPeriodic: Omitted

rb_MappingInfo:

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

dch: 5

logicalChannelIdentity: 3

rlc_SizeList:

configured: NULL

mac_LogicalChannelPriority: 3

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

dch: 10

logicalChannelIdentity: 3

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

rach: NULL

logicalChannelIdentity: 3

rlc_SizeList:

explicitList:

RLC_SizeExplicitList.element:

rlc_SizeIndex: 1

mac_LogicalChannelPriority: 3

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

fach: NULL

logicalChannelIdentity: 3

SRB_InformationSetupList2.element:

rb_Identity: Omitted

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard: dat15_MaxDAT [enum=10]

transmissionWindowSize: tw32_TransmissionWindowSize [enum=3]

timerRST: tr500_TimerRST [enum=9]

max_RST: rst1_MaxRST [enum=0]

pollingInfo:

timerPollProhibit: tpp200_TimerPollProhibit [enum=19]

timerPoll: tp200_TimerPoll [enum=19]

poll_PDU: Omitted

poll_SDU: sdu1_Poll_SDU [enum=0]

lastTransmissionPDU_Poll: 1

lastRetransmissionPDU_Poll: 1

pollWindow: pw99_PollWindow [enum=7]

timerPollPeriodic: Omitted

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery: 1

receivingWindowSize: rw32_ReceivingWindowSize [enum=3]

dl_RLC_StatusInfo:

timerStatusProhibit: tsp200_TimerStatusProhibit [enum=19]

timerEPC: Omitted

missingPDU_Indicator: 1

timerStatusPeriodic: Omitted

rb_MappingInfo:

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

dch: 5

logicalChannelIdentity: 4

rlc_SizeList:

configured: NULL

mac_LogicalChannelPriority: 4

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

dch: 10

logicalChannelIdentity: 4

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

rach: NULL

logicalChannelIdentity: 4

rlc_SizeList:

explicitList:

RLC_SizeExplicitList.element:

rlc_SizeIndex: 1

mac_LogicalChannelPriority: 4

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

fach: NULL

logicalChannelIdentity: 4

ul_CommonTransChInfo:

tfc_Subset: Omitted

prach_TFCS: Omitted

modeSpecificInfo:

fdd:

ul_TFCS:

normalTFCI_Signalling:

complete:

ctfcSize:

ctfc2Bit:

ctfc2Bit.noName:

ctfc2: 0

powerOffsetInformation:

gainFactorInformation:

computedGainFactors: 0

powerOffsetPp_m: Omitted

ctfc2Bit.noName:

ctfc2: 1

powerOffsetInformation:

gainFactorInformation:

signalledGainFactors:

modeSpecificInfo:

fdd:

gainFactorBetaC: 11

gainFactorBetaD: 15

referenceTFC_ID: 0

powerOffsetPp_m: Omitted

ul_AddReconfTransChInfoList:

UL_AddReconfTransChInfoList.element:

ul_TransportChannelType: dch_UL_TrCH_Type [enum=0]

transportChannelIdentity: 5

transportFormatSet:

dedicatedTransChTFS:

tti:

tti10:

DedicatedDynamicTF_InfoList.element:

rlc_Size:

bitMode:

sizeType2:

part1: 2

part2: Omitted

numberOfTbSizeList:

numberOfTbSizeList.element:

zero: NULL

numberOfTbSizeList.element:

one: NULL

logicalChannelList:

allSizes: NULL

semistaticTF_Information:

channelCodingType:

convolutional: third_CodingRate [enum=1]

rateMatchingAttribute: 192

crc_Size: crc16_CRC_Size [enum=3]

dl_CommonTransChInfo:

sccpch_TFCS: Omitted

modeSpecificInfo:

fdd:

dl_Parameters:

sameAsUL: NULL

dl_AddReconfTransChInfoList:

DL_AddReconfTransChInfoList.element:

dl_TransportChannelType: dch_DL_TrCH_Type [enum=0]

dl_transportChannelIdentity: 10

tfs_SignallingMode:

sameAsULTrCH:

ul_TransportChannelType: dch_UL_TrCH_Type [enum=0]

ul_TransportChannelIdentity: 5

dch_QualityTarget:

bler_QualityValue: -20

dummy: Omitted

frequencyInfo: Omitted

maxAllowedUL_TX_Power: Omitted

ul_ChannelRequirement:

ul_DPCH_Info:

ul_DPCH_PowerControlInfo:

fdd:

dpcch_PowerOffset: -40

pc_Preamble: 1

sRB_delay: 7

powerControlAlgorithm:

algorithm1: 0

modeSpecificInfo:

fdd:

scramblingCodeType: longSC_ScramblingCodeType [enum=1]

scramblingCode: 0

numberOfDPDCH: Default

spreadingFactor: sf64_SpreadingFactor [enum=4]

tfci_Existence: 1

numberOfFBI_Bits: Omitted

puncturingLimit: pl1_PuncturingLimit [enum=15]

dl_CommonInformation:

dl_DPCH_InfoCommon:

cfnHandling:

initialise:

cfntargetsfnframeoffset: Omitted

modeSpecificInfo:

fdd:

dl_DPCH_PowerControlInfo:

modeSpecificInfo:

fdd:

dpc_Mode: singleTPC_DPC_Mode [enum=0]

powerOffsetPilot_pdpdch: 0

dl_rate_matching_restriction: Omitted

spreadingFactorAndPilot:

sfd128: pb4_PilotBits128 [enum=0]

positionFixedOrFlexible: fixed_PositionFixedOrFlexible [enum=0]

tfci_Existence: 0

modeSpecificInfo:

fdd:

defaultDPCH_OffsetValue: 0

dpch_CompressedModeInfo: Omitted

tx_DiversityMode: noDiversity_TX_DiversityMode [enum=0]

ssdt_Information: Omitted

dl_InformationPerRL_List:

DL_InformationPerRL_List.element:

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode: 100

pdsch_SHO_DCH_Info: Omitted

pdsch_CodeMapping: Omitted

dl_DPCH_InfoPerRL:

fdd:

pCPICH_UsageForChannelEst: mayBeUsed_PCPICH_UsageForChannelEst [enum=0]

dpch_FrameOffset: 0

secondaryCPICH_Info: Omitted

dl_ChannelisationCodeList:

DL_ChannelisationCodeList.element:

secondaryScramblingCode: 1

sf_AndCodeNumber:

sf128: 0

scramblingCodeChange: noCodeChange_ScramblingCodeChange [enum=1]

tpc_CombinationIndex: 0

ssdt_CellIdentity: Omitted

closedLoopTimingAdjMode: Omitted

sccpch_InfoforFACH: Omitted

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]30 E7 22 24 46 68 80 02
[8]01 00 01 00 04 00 00 4D
[16]82 69 3A 10 10 89 0D 42
[24]00 02 81 9E 8E 46 C9 A6
[32]7C 9C 4E 74 20 A5 12 3A
[40]8C 00 15 13 3D 1C 8D 93
[48]4C F9 38 9C E8 42 52 24
[56]B5 28 00 4A 46 7A 39 1B
[64]26 99 F2 71 39 D0 86 B4
[72]49 EA 70 00 D4 C8 00 06
[80]25 2B F0 02 00 08 82 23
[88]BF 66 08 98 95 A5 47 82
[96]00 00 01 3F 90 0A 14 00
[104]02 06 40 00 0C 28 08

#### MAC_DATA_REQ

RLC MAC @ 00:07:20.660

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: CCCH
CFN: 43

Message Details:

RLC PDU size (bits):160
RLC PDU (raw):

[0]25 F8 30 E7 22 24 46 68
[8]80 02 01 00 01 00 04 00
[16]00 4D 82 69

RLC PDU (decoded):

Sequence number:18
Length indicator 0 (octets):124 (the first data octet in this RLC PDU is the first octet of a RLC SDU)
Segment associated with length indicator 0 (0 octets):

Last segment, not associated with any length indicators (18 octets):

[0]30 E7 22 24 46 68 80 02
[8]01 00 01 00 04 00 00 4D
[16]82 69

#### MAC_DATA_REQ

RLC MAC @ 00:07:20.660

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: CCCH
CFN: 43

Message Details:

RLC PDU size (bits):160
RLC PDU (raw):

[0]26 3A 10 10 89 0D 42 00
[8]02 81 9E 8E 46 C9 A6 7C
[16]9C 4E 74 20

RLC PDU (decoded):

Sequence number:19
Last segment, not associated with any length indicators (19 octets):

[0]3A 10 10 89 0D 42 00 02
[8]81 9E 8E 46 C9 A6 7C 9C
[16]4E 74 20

#### MAC_DATA_REQ

RLC MAC @ 00:07:20.660

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: CCCH
CFN: 43

Message Details:

RLC PDU size (bits):160
RLC PDU (raw):

[0]28 A5 12 3A 8C 00 15 13
[8]3D 1C 8D 93 4C F9 38 9C
[16]E8 42 52 24

RLC PDU (decoded):

Sequence number:20
Last segment, not associated with any length indicators (19 octets):

[0]A5 12 3A 8C 00 15 13 3D
[8]1C 8D 93 4C F9 38 9C E8
[16]42 52 24

#### MAC_DATA_REQ

RLC MAC @ 00:07:20.660

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: CCCH
CFN: 43

Message Details:

RLC PDU size (bits):160
RLC PDU (raw):

[0]2A B5 28 00 4A 46 7A 39
[8]1B 26 99 F2 71 39 D0 86
[16]B4 49 EA 70

RLC PDU (decoded):

Sequence number:21
Last segment, not associated with any length indicators (19 octets):

[0]B5 28 00 4A 46 7A 39 1B
[8]26 99 F2 71 39 D0 86 B4
[16]49 EA 70

#### MAC_DATA_REQ

RLC MAC @ 00:07:20.660

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: CCCH
CFN: 43

Message Details:

RLC PDU size (bits):160
RLC PDU (raw):

[0]2C 00 D4 C8 00 06 25 2B
[8]F0 02 00 08 82 23 BF 66
[16]08 98 95 A5

RLC PDU (decoded):

Sequence number:22
Last segment, not associated with any length indicators (19 octets):

[0]00 D4 C8 00 06 25 2B F0
[8]02 00 08 82 23 BF 66 08
[16]98 95 A5

#### MAC_DATA_REQ

RLC MAC @ 00:07:20.660

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: CCCH
CFN: 43

Message Details:

RLC PDU size (bits):160
RLC PDU (raw):

[0]2F 23 FE 47 82 00 00 01
[8]3F 90 0A 14 00 02 06 40
[16]00 0C 28 08

RLC PDU (decoded):

Sequence number:23
Length indicator 0 (octets):17
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (17 octets):

[0]47 82 00 00 01 3F 90 0A
[8]14 00 02 06 40 00 0C 28
[16]08
Padding associated with length indicator 1 (0 octets):

#### PHY_DATA_REQ

MAC PHY @ 00:07:20.660

BTS unit: 1:1
Channel No: 0 Name: FACH
CFN: 43

Message Details:

TFI:2
TB set size:336
TB size:168
TB set (raw, each TB word aligned):

[0]40 25 F8 30 E7 22 24 46
[8]68 80 02 01 00 01 00 04
[16]00 00 4D 82 69 00 40 26
[24]3A 10 10 89 0D 42 00 02
[32]81 9E 8E 46 C9 A6 7C 9C
[40]4E 74 20 00

TB set (decoded):

TB 0:

TCTF:64
MAC SDU (160 bits):

[0]25 F8 30 E7 22 24 46 68
[8]80 02 01 00 01 00 04 00
[16]00 4D 82 69

TB 1:

TCTF:64
MAC SDU (160 bits):

[0]26 3A 10 10 89 0D 42 00
[8]02 81 9E 8E 46 C9 A6 7C
[16]9C 4E 74 20

#### PHY_DATA_REQ

MAC PHY @ 00:07:20.670

BTS unit: 1:1
Channel No: 0 Name: FACH
CFN: 44

Message Details:

TFI:2
TB set size:336
TB size:168
TB set (raw, each TB word aligned):

[0]40 28 A5 12 3A 8C 00 15
[8]13 3D 1C 8D 93 4C F9 38
[16]9C E8 42 52 24 00 40 2A
[24]B5 28 00 4A 46 7A 39 1B
[32]26 99 F2 71 39 D0 86 B4
[40]49 EA 70 00

TB set (decoded):

TB 0:

TCTF:64
MAC SDU (160 bits):

[0]28 A5 12 3A 8C 00 15 13
[8]3D 1C 8D 93 4C F9 38 9C
[16]E8 42 52 24

TB 1:

TCTF:64
MAC SDU (160 bits):

[0]2A B5 28 00 4A 46 7A 39
[8]1B 26 99 F2 71 39 D0 86
[16]B4 49 EA 70

#### PHY_DATA_REQ

MAC PHY @ 00:07:20.680

BTS unit: 1:1
Channel No: 0 Name: FACH
CFN: 45

Message Details:

TFI:2
TB set size:336
TB size:168
TB set (raw, each TB word aligned):

[0]40 2C 00 D4 C8 00 06 25
[8]2B F0 02 00 08 82 23 BF
[16]66 08 98 95 A5 00 40 2F
[24]23 FE 47 82 00 00 01 3F
[32]90 0A 14 00 02 06 40 00
[40]0C 28 08 00

TB set (decoded):

TB 0:

TCTF:64
MAC SDU (160 bits):

[0]2C 00 D4 C8 00 06 25 2B
[8]F0 02 00 08 82 23 BF 66
[16]08 98 95 A5

TB 1:

TCTF:64
MAC SDU (160 bits):

[0]2F 23 FE 47 82 00 00 01
[8]3F 90 0A 14 00 02 06 40
[16]00 0C 28 08

#### CPHY_SYNC_IND

PHY RRC @ 00:07:20.890

BTS unit: 1:1
Channel No: 0 Name: U_DPCH
CFN: 66

Message Details:

#### PHY_DATA_IND

PHY MAC @ 00:07:21.060

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 63

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 00 04 B0 C0 00 08 00
[8]00 51 1B 8D D0 6A 4C 66
[16]88 A2 C0 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 00 4B 0C 00 00 80 00
[8]05 11 B8 DD 06 A4 C6 68
[16]8A 2C

#### MAC_DATA_IND

MAC RLC @ 00:07:21.060

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 63

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 00 4B 0C 00 00 80 00
[8]05 11 B8 DD 06 A4 C6 68
[16]8A 2C

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:0
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]4B 0C 00 00 80 00 05 11
[8]B8 DD 06 A4 C6 68 8A 2C

#### PHY_DATA_IND

PHY MAC @ 00:07:21.070

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 64

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 00 88 30 34 80 01 80
[8]01 18 FC FC 0C C0 D5 C6
[16]28 48 C0 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 08 83 03 48 00 18 00
[8]11 8F CF C0 CC 0D 5C 62
[16]84 8C

#### MAC_DATA_IND

MAC RLC @ 00:07:21.070

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 64

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 08 83 03 48 00 18 00
[8]11 8F CF C0 CC 0D 5C 62
[16]84 8C

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:1
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]83 03 48 00 18 00 11 8F
[8]CF C0 CC 0D 5C 62 84 8C

#### PHY_DATA_IND

PHY MAC @ 00:07:21.080

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 65

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 01 50 BF E0 28 99 01
[8]00 05 55 55 55 55 55 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 15 0B FE 02 89 90 10
[8]00 55 55 55 55 55 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:07:21.080

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 65

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 15 0B FE 02 89 90 10
[8]00 55 55 55 55 55 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:2
Polling bit:1 (request a status report)
Length indicator 0 (octets):5
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (5 octets):

[0]02 89 90 10 00
Padding associated with length indicator 1 (9 octets):

[0]55 55 55 55 55 55 55 55
[8]55

#### MAC_DATA_REQ

RLC MAC @ 00:07:21.090

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 86

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:3

#### PHY_DATA_REQ

MAC PHY @ 00:07:21.090

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 86

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]10 20 03 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:07:21.090

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 66

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 00 01 58 21 D0 16 04
[8]04 09 80 78 88 00 00 82
[16]85 8A F0 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 00 15 82 1D 01 60 40
[8]40 98 07 88 80 00 08 28
[16]58 AF

#### MAC_DATA_IND

MAC RLC @ 00:07:21.090

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 66

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 00 15 82 1D 01 60 40
[8]40 98 07 88 80 00 08 28
[16]58 AF

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:0
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]15 82 1D 01 60 40 40 98
[8]07 88 80 00 08 28 58 AF

#### PHY_DATA_IND

PHY MAC @ 00:07:21.100

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 67

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 00 89 C1 19 AA 15 19
[8]93 22 50 CC 0C D5 89 1B
[16]8B 8B 10 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 08 9C 11 9A A1 51 99
[8]32 25 0C C0 CD 58 91 B8
[16]B8 B1

#### MAC_DATA_IND

MAC RLC @ 00:07:21.100

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 67

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 08 9C 11 9A A1 51 99
[8]32 25 0C C0 CD 58 91 B8
[16]B8 B1

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:1
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]9C 11 9A A1 51 99 32 25
[8]0C C0 CD 58 91 B8 B8 B1

#### PHY_DATA_IND

PHY MAC @ 00:07:21.110

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 68

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 01 03 83 82 0C 02 FA
[8]04 C3 B2 A1 98 81 72 A0
[16]19 01 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 10 38 38 20 C0 2F A0
[8]4C 3B 2A 19 88 17 2A 01
[16]90 10

#### MAC_DATA_IND

MAC RLC @ 00:07:21.110

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 68

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 10 38 38 20 C0 2F A0
[8]4C 3B 2A 19 88 17 2A 01
[16]90 10

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:2
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]38 38 20 C0 2F A0 4C 3B
[8]2A 19 88 17 2A 01 90 10

#### PHY_DATA_IND

PHY MAC @ 00:07:21.120

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 69

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 01 D0 BF E0 00 20 00
[8]04 05 55 55 55 55 55 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 1D 0B FE 00 02 00 00
[8]40 55 55 55 55 55 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:07:21.120

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 69

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 1D 0B FE 00 02 00 00
[8]40 55 55 55 55 55 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:3
Polling bit:1 (request a status report)
Length indicator 0 (octets):5
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (5 octets):

[0]00 02 00 00 40
Padding associated with length indicator 1 (9 octets):

[0]55 55 55 55 55 55 55 55
[8]55

#### RLC_AM_DATA_IND: rrcConnectionSetupComplete

RLC LLA @ 00:07:21.130

Channel No: 2 Name: DCCH

Message Details:

UL_DCCH_Message:

integrityCheckInfo: Omitted

message:

rrcConnectionSetupComplete:

rrc_TransactionIdentifier: 0

startList:

STARTList.element:

cn_DomainIdentity: ps_domain_CN_DomainIdentity [enum=1]

start_Value: 00000000000000000010

STARTList.element:

cn_DomainIdentity: cs_domain_CN_DomainIdentity [enum=0]

start_Value: 00000000000000000010

ue_RadioAccessCapability:

accessStratumReleaseIndicator: r99_AccessStratumReleaseIndicator [enum=0]

pdcp_Capability:

losslessSRNS_RelocationSupport: 0

supportForRfc2507:

notSupported: NULL

rlc_Capability:

totalRLC_AM_BufferSize: kb50_TotalRLC_AM_BufferSize [enum=2]

maximumRLC_WindowSize: mws2047_MaximumRLC_WindowSize [enum=0]

maximumAM_EntityNumber: am6_MaximumAM_EntityNumberRLC_Cap [enum=3]

transportChannelCapability:

dl_TransChCapability:

maxNoBitsReceived: b8960_MaxNoBits [enum=7]

maxConvCodeBitsReceived: b1280_MaxNoBits [enum=1]

turboDecodingSupport:

supported: b8960_MaxNoBits [enum=7]

maxSimultaneousTransChs: e8_MaxSimultaneousTransChsDL [enum=1]

maxSimultaneousCCTrCH_Count: 1

maxReceivedTransportBlocks: tb32_MaxTransportBlocksDL [enum=3]

maxNumberOfTFC: tfc128_MaxNumberOfTFC_DL [enum=5]

maxNumberOfTF: tf64_MaxNumberOfTF [enum=1]

ul_TransChCapability:

maxNoBitsTransmitted: b3840_MaxNoBits [enum=3]

maxConvCodeBitsTransmitted: b1280_MaxNoBits [enum=1]

turboEncodingSupport:

supported: b3840_MaxNoBits [enum=3]

maxSimultaneousTransChs: e8_MaxSimultaneousTransChsUL [enum=2]

modeSpecificInfo:

fdd: NULL

maxTransmittedBlocks: tb32_MaxTransportBlocksUL [enum=4]

maxNumberOfTFC: tfc64_MaxNumberOfTFC_UL [enum=5]

maxNumberOfTF: tf32_MaxNumberOfTF [enum=0]

rf_Capability:

fddRF_Capability:

ue_PowerClass: 4

txRxFrequencySeparation: mhz190_TxRxFrequencySeparation [enum=0]

tddRF_Capability: Omitted

physicalChannelCapability:

fddPhysChCapability:

downlinkPhysChCapability:

maxNoDPCH_PDSCH_Codes: 1

maxNoPhysChBitsReceived: b9600_MaxNoPhysChBitsReceived [enum=6]

supportForSF_512: 0

supportOfPDSCH: 0

simultaneousSCCPCH_DPCH_Reception:

notSupported: NULL

uplinkPhysChCapability:

maxNoDPDCH_BitsTransmitted: b4800_MaxNoDPDCH_BitsTransmitted [enum=3]

supportOfPCPCH: 0

tddPhysChCapability: Omitted

ue_MultiModeRAT_Capability:

multiRAT_CapabilityList:

supportOfGSM: 1

supportOfMulticarrier: 0

multiModeCapability: fdd_MultiModeCapability [enum=1]

securityCapability:

cipheringAlgorithmCap: 0000000000000011

integrityProtectionAlgorithmCap: 0000000000000010

ue_positioning_Capability:

standaloneLocMethodsSupported: 0

ue_BasedOTDOA_Supported: 0

networkAssistedGPS_Supported: noNetworkAssistedGPS_NetworkAssistedGPS_Supported [enum=3]

supportForUE_GPS_TimingOfCellFrames: 0

supportForIPDL: 0

measurementCapability:

downlinkCompressedMode:

fdd_Measurements: 1

tdd_Measurements: Omitted

gsm_Measurements:

gsm900: 1

dcs1800: 1

gsm1900: 1

multiCarrierMeasurements: 0

uplinkCompressedMode:

fdd_Measurements: 1

tdd_Measurements: Omitted

gsm_Measurements:

gsm900: 1

dcs1800: 1

gsm1900: 1

multiCarrierMeasurements: 0

ue_RATSpecificCapability:

InterRAT_UE_RadioAccessCapabilityList.element:

gsm:

gsm_Classmark2: 33035718A1

gsm_Classmark3: 60144C8080

v370NonCriticalExtensions: Omitted

Layer 3 SDU:

[0]4B 0C 00 00 80 00 05 11
[8]B8 DD 06 A4 C6 68 8A 2C
[16]83 03 48 00 18 00 11 8F
[24]CF C0 CC 0D 5C 62 84 8C
[32]02 89 90 10 00

#### RLC_AM_DATA_IND

LLA RRC @ 00:07:21.130

Channel ID: Rb2
Cell ID: -1

Message Details:

RLC_AM_DATA_IND:

cellId:-1

routingInfo:

rB_Identity:2

integrityResult:

integrityUsed (IntegrityStatus):i_pass

aM_message:

uL_DCCH_Message:

integrityCheckInfo: Omit

message: (UL_DCCH_MessageType)

rrcConnectionSetupComplete:

rrc_TransactionIdentifier:0

startList:

STARTSingle:

cn_DomainIdentity:ps_domain
start_Value:00000000000000000010

STARTSingle:

cn_DomainIdentity:cs_domain
start_Value:00000000000000000010

ue_RadioAccessCapability:

accessStratumReleaseIndicator:r99

pdcp_Capability:

losslessSRNS_RelocationSupport:false

supportForRfc2507:

notSupported:

rlc_Capability:

totalRLC_AM_BufferSize:kb50
maximumRLC_WindowSize:mws2047
maximumAM_EntityNumber (MaximumAM_EntityNumberRLC_Cap):am6

transportChannelCapability:

dl_TransChCapability:

maxNoBitsReceived (MaxNoBits):b8960
maxConvCodeBitsReceived (MaxNoBits):b1280

turboDecodingSupport: (TurboSupport)

supported (MaxNoBits):b8960

maxSimultaneousTransChs (MaxSimultaneousTransChsDL):e8
maxSimultaneousCCTrCH_Count:1
maxReceivedTransportBlocks (MaxTransportBlocksDL):tb32
maxNumberOfTFC (MaxNumberOfTFC_DL):tfc128
maxNumberOfTF:tf64

ul_TransChCapability:

maxNoBitsTransmitted (MaxNoBits):b3840
maxConvCodeBitsTransmitted (MaxNoBits):b1280

turboEncodingSupport: (TurboSupport)

supported (MaxNoBits):b3840

maxSimultaneousTransChs (MaxSimultaneousTransChsUL):e8

modeSpecificInfo:

fdd:

maxTransmittedBlocks (MaxTransportBlocksUL):tb32
maxNumberOfTFC (MaxNumberOfTFC_UL):tfc64
maxNumberOfTF:tf32

rf_Capability:

fddRF_Capability:

ue_PowerClass:4
txRxFrequencySeparation:mhz190

tddRF_Capability: Omit

physicalChannelCapability:

fddPhysChCapability:

downlinkPhysChCapability: (DL_PhysChCapabilityFDD)

maxNoDPCH_PDSCH_Codes:1
maxNoPhysChBitsReceived:b9600
supportForSF_512:false
supportOfPDSCH:false

simultaneousSCCPCH_DPCH_Reception:

notSupported:

uplinkPhysChCapability: (UL_PhysChCapabilityFDD)

maxNoDPDCH_BitsTransmitted:b4800
supportOfPCPCH:false

tddPhysChCapability: Omit

ue_MultiModeRAT_Capability:

multiRAT_CapabilityList: (MultiRAT_Capability)

supportOfGSM:true
supportOfMulticarrier:false

multiModeCapability:fdd

securityCapability:

cipheringAlgorithmCap:0000000000000011
integrityProtectionAlgorithmCap:0000000000000010

ue_positioning_Capability:

standaloneLocMethodsSupported:false
ue_BasedOTDOA_Supported:false
networkAssistedGPS_Supported:noNetworkAssistedGPS
supportForUE_GPS_TimingOfCellFrames:false
supportForIPDL:false

measurementCapability:

downlinkCompressedMode: (CompressedModeMeasCapability)

fdd_Measurements:true
tdd_Measurements: Omit

gsm_Measurements:

gsm900:true
dcs1800:true
gsm1900:true

multiCarrierMeasurements:false

uplinkCompressedMode: (CompressedModeMeasCapability)

fdd_Measurements:true
tdd_Measurements: Omit

gsm_Measurements:

gsm900:true
dcs1800:true
gsm1900:true

multiCarrierMeasurements:false

ue_RATSpecificCapability: (InterRAT_UE_RadioAccessCapabilityList)

InterRAT_UE_RadioAccessCapability:

gsm:

gsm_Classmark2:

[0]33 03 57 18 A1
gsm_Classmark3:

[0]60 14 4C 80 80

v370NonCriticalExtensions: Omit

#### RLC_AM_DATA_IND: initialDirectTransfer

RLC RRC @ 00:07:21.130

Channel No: 3 Name: DCCH

Message Details:

UL_DCCH_Message:

integrityCheckInfo: Omitted

message:

initialDirectTransfer:

cn_DomainIdentity: ps_domain_CN_DomainIdentity [enum=1]

intraDomainNasNodeSelector:

version:

release99:

cn_Type:

gsm_Map_IDNNS:

routingbasis:

localPTMSI:

routingparameter: 1000011101

enteredparameter: 0

nas_Message: 08081300F1100001050B15F38233542A332644A19819AB123717162707041805F4098765433102E54032020000

measuredResultsOnRACH: Omitted

v3a0NonCriticalExtensions:

initialDirectTransfer_v3a0ext:

start_Value: 00000000000000000010

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]15 82 1D 01 60 40 40 98
[8]07 88 80 00 08 28 58 AF
[16]9C 11 9A A1 51 99 32 25
[24]0C C0 CD 58 91 B8 B8 B1
[32]38 38 20 C0 2F A0 4C 3B
[40]2A 19 88 17 2A 01 90 10
[48]00 02 00 00 40

#### RRC_DATA_IND: gmm:routingAreaUpdateRequest

RRC NAS @ 00:07:21.130

Cell ID: -1

Message Details:

ROUTINGAREAUPDATEREQUEST:

skipIndicator: 0000

gMMProtocolDiscriminator: 1000

msgType: 00001000

gprsCiphKeySeqNo:

spare1: 0

keySeq: 001

updateType:

for: 0

value: 011

oldRAI:

plmn: 00F110

lac: 0001

rac: 05

msRadioAccessCap:

iel: 0B

value: 15F38233542A332644A198

oldPTMSI_Signature:

iei: 00011001

value: AB1237

readyTimer:

iei: 00010111

unit: 000

value: 10110

drxParameter:

iei: 00100111

splitPGcycleCode: 00000111

cnDRXcoef: 0000

splitOnCCCH: 0

nonDRXtimer: 100

tmsiStatus: Omitted

ptmsi:

iei: 00011000

iel: 05

iDigit1: 1111

oddEvenInd: 0

typeOfId: 100

otherDigits: 09876543

msnetworkcap:

iei: 00110001

iel: 02

value: E540

pDP_ContextStatus:

iei: 00110010

iel: 02

nSAPI: 0000000000000000

#### MAC_DATA_REQ

RLC MAC @ 00:07:21.130

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 90

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 40 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:4

#### PHY_DATA_REQ

MAC PHY @ 00:07:21.130

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 90

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 04 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 40 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### RRC_DATA_REQ: gmm:routingAreaUpdateReject

NAS RRC @ 00:07:21.160

Cell ID: -1

Message Details:

ROUTING_AREA_UPDATE_REJECT:

skipIndicator: 0000

gMMProtocolDiscriminator: 1000

msgType: 00001011

gmmCause: 0E

spare: 0000

forceToStandby:

spare: 0

value: 000

t3302Value: Omitted

#### RLC_AM_DATA_REQ:downlinkDirectTransfer

RRC RLC @ 00:07:21.160

Channel No: 3 Name: DCCH

Message Details:

Opt1: 0

Opt2: 0

DL_DCCH_Message:

integrityCheckInfo: Omitted

message:

downlinkDirectTransfer:

r3:

downlinkDirectTransfer_r3:

rrc_TransactionIdentifier: 0

cn_DomainIdentity: ps_domain_CN_DomainIdentity [enum=1]

nas_Message: 080B0E00

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]14 20 06 10 16 1C 00

#### MAC_DATA_REQ

RLC MAC @ 00:07:21.160

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 93

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 05 0F FE 14 20 06 10
[8]16 1C 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:0
Polling bit:1 (request a status report)
Length indicator 0 (octets):7
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (7 octets):

[0]14 20 06 10 16 1C 00
Padding associated with length indicator 1 (7 octets):

[0]00 00 00 00 00 00 00

#### PHY_DATA_REQ

MAC PHY @ 00:07:21.160

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 93

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 00 50 FF E1 42 00 61
[8]01 61 C0 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 05 0F FE 14 20 06 10
[8]16 1C 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:07:21.290

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 86

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 01 50 BF E0 28 99 01
[8]00 05 55 55 55 55 55 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 15 0B FE 02 89 90 10
[8]00 55 55 55 55 55 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:07:21.290

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 86

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 15 0B FE 02 89 90 10
[8]00 55 55 55 55 55 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:2
Polling bit:1 (request a status report)
Length indicator 0 (octets):5
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (5 octets):

[0]02 89 90 10 00
Padding associated with length indicator 1 (9 octets):

[0]55 55 55 55 55 55 55 55
[8]55

#### MAC_DATA_REQ

RLC MAC @ 00:07:21.300

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 107

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:3

#### PHY_DATA_REQ

MAC PHY @ 00:07:21.300

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 107

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]10 20 03 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:07:21.330

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 90

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 01 D0 BF E0 00 20 00
[8]04 05 55 55 55 55 55 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 1D 0B FE 00 02 00 00
[8]40 55 55 55 55 55 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:07:21.330

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 90

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 1D 0B FE 00 02 00 00
[8]40 55 55 55 55 55 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:3
Polling bit:1 (request a status report)
Length indicator 0 (octets):5
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (5 octets):

[0]00 02 00 00 40
Padding associated with length indicator 1 (9 octets):

[0]55 55 55 55 55 55 55 55
[8]55

#### MAC_DATA_REQ

RLC MAC @ 00:07:21.340

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 111

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 40 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:4

#### PHY_DATA_REQ

MAC PHY @ 00:07:21.340

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 111

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 04 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 40 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### MAC_DATA_REQ

RLC MAC @ 00:07:21.360

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 113

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 05 0F FE 14 20 06 10
[8]16 1C 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:0
Polling bit:1 (request a status report)
Length indicator 0 (octets):7
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (7 octets):

[0]14 20 06 10 16 1C 00
Padding associated with length indicator 1 (7 octets):

[0]00 00 00 00 00 00 00

#### PHY_DATA_REQ

MAC PHY @ 00:07:21.360

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 113

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 00 50 FF E1 42 00 61
[8]01 61 C0 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 05 0F FE 14 20 06 10
[8]16 1C 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:07:21.390

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 96

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 01 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 10 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### MAC_DATA_IND

MAC RLC @ 00:07:21.390

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 96

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 10 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:1

#### PHY_DATA_IND

PHY MAC @ 00:07:21.600

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 117

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 01 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 10 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### MAC_DATA_IND

MAC RLC @ 00:07:21.600

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 117

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 10 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:1

#### MAC_DATA_REQ

RLC MAC @ 00:07:22.170

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 194

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]01 07 FE 3C 80 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

Sequence number:0
Length indicator 0 (octets):3
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (3 octets):

[0]3C 80 00
Padding associated with length indicator 1 (12 octets):

[0]00 00 00 00 00 00 00 00
[8]00 00 00 00

#### PHY_DATA_REQ

MAC PHY @ 00:07:22.170

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 194

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]00 10 7F E3 C8 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:0
MAC SDU (144 bits):

[0]01 07 FE 3C 80 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### RLC_UM_DATA_REQ

RRC LLA @ 00:07:22.180

Channel ID: Rb1
Cell ID: -1

Message Details:

RLC_UM_DATA_REQ:

cellId:-1

routingInfo:

rB_Identity:1

uM_message:

dL_DCCH_Message:

integrityCheckInfo: Omit

message: (DL_DCCH_MessageType)

rrcConnectionRelease:

r3:

rrcConnectionRelease_r3: (RRCConnectionRelease_r3_IEs)

rrc_TransactionIdentifier:0
n_308:1
releaseCause:normalEvent

rplmn_information: Omit

laterNonCriticalExtensions: Omit

specialLI:false

#### RLC_UM_DATA_REQ: rrcConnectionRelease

LLA RLC @ 00:07:22.180

Channel No: 1 Name: DCCH

Message Details:

DL_DCCH_Message:

integrityCheckInfo: Omitted

message:

rrcConnectionRelease:

r3:

rrcConnectionRelease_r3:

rrc_TransactionIdentifier: 0

n_308: 1

releaseCause: normalEvent_ReleaseCause [enum=0]

rplmn_information: Omitted

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]3C 80 00

#### PHY_DATA_IND

PHY MAC @ 00:07:22.410

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 198

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]00 10 5F E4 40 05 55 55
[8]55 55 55 55 55 55 55 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:0
MAC SDU (144 bits):

[0]01 05 FE 44 00 55 55 55
[8]55 55 55 55 55 55 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:07:22.410

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 198

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]01 05 FE 44 00 55 55 55
[8]55 55 55 55 55 55 55 55
[16]55 55

RLC PDU (decoded):

Sequence number:0
Length indicator 0 (octets):2
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (2 octets):

[0]44 00
Padding associated with length indicator 1 (13 octets):

[0]55 55 55 55 55 55 55 55
[8]55 55 55 55 55

#### RLC_UM_DATA_IND: rrcConnectionReleaseComplete

RLC LLA @ 00:07:22.440

Channel No: 1 Name: DCCH

Message Details:

UL_DCCH_Message:

integrityCheckInfo: Omitted

message:

rrcConnectionReleaseComplete:

rrc_TransactionIdentifier: 0

errorIndication: Omitted

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]44 00

#### RLC_UM_DATA_IND

LLA RRC @ 00:07:22.440

Channel ID: Rb1
Cell ID: -1

Message Details:

RLC_UM_DATA_IND:

cellId:-1

routingInfo:

rB_Identity:1

integrityResult:

integrityUsed (IntegrityStatus):i_pass

uM_message:

uL_DCCH_Message:

integrityCheckInfo: Omit

message: (UL_DCCH_MessageType)

rrcConnectionReleaseComplete:

rrc_TransactionIdentifier:0

errorIndication: (FailureCauseWithProtErr) Omit

laterNonCriticalExtensions: Omit

#### PHY_DATA_IND

PHY MAC @ 00:07:22.570

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 214

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]00 30 5F E4 40 05 55 55
[8]55 55 55 55 55 55 55 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:0
MAC SDU (144 bits):

[0]03 05 FE 44 00 55 55 55
[8]55 55 55 55 55 55 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:07:22.570

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 214

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]03 05 FE 44 00 55 55 55
[8]55 55 55 55 55 55 55 55
[16]55 55

RLC PDU (decoded):

Sequence number:1
Length indicator 0 (octets):2
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (2 octets):

[0]44 00
Padding associated with length indicator 1 (13 octets):

[0]55 55 55 55 55 55 55 55
[8]55 55 55 55 55

#### CRLC UM Channel Release REQ

LLA RLC @ 00:07:22.610

BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 238

Message Details:

#### CRLC UM Channel Release CNF

RLC LLA @ 00:07:22.610

BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 238

Message Details:

#### RLC_UM_DATA_IND: rrcConnectionReleaseComplete

RLC LLA @ 00:07:22.610

Channel No: 1 Name: DCCH

Message Details:

UL_DCCH_Message:

integrityCheckInfo: Omitted

message:

rrcConnectionReleaseComplete:

rrc_TransactionIdentifier: 0

errorIndication: Omitted

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]44 00

#### RLC_UM_DATA_IND

LLA RRC @ 00:07:22.610

Channel ID: Rb1
Cell ID: -1

Message Details:

RLC_UM_DATA_IND:

cellId:-1

routingInfo:

rB_Identity:1

integrityResult:

integrityUsed (IntegrityStatus):i_pass

uM_message:

uL_DCCH_Message:

integrityCheckInfo: Omit

message: (UL_DCCH_MessageType)

rrcConnectionReleaseComplete:

rrc_TransactionIdentifier:0

errorIndication: (FailureCauseWithProtErr) Omit

laterNonCriticalExtensions: Omit

#### CRLC_Config_REQ

RRC LLA @ 00:07:22.610

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:1

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC AM Channel Release REQ

LLA RLC @ 00:07:22.620

BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 239

Message Details:

#### CRLC AM Channel Release CNF

RLC LLA @ 00:07:22.620

BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 239

Message Details:

#### CPHY_OUTSYNC_IND

PHY RRC @ 00:07:22.630

BTS unit: 1:1
Channel No: 0 Name: U_DPCH
CFN: 240

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:07:22.630

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:1

#### CRLC_Config_REQ

RRC LLA @ 00:07:22.630

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:2

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC_Config_CNF

LLA RRC @ 00:07:22.640

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:2

#### CRLC_Config_REQ

RRC LLA @ 00:07:22.640

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:3

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC AM Channel Release REQ

LLA RLC @ 00:07:22.640

BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 241

Message Details:

#### CRLC AM Channel Release CNF

RLC LLA @ 00:07:22.640

BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 241

Message Details:

#### CRLC AM Channel Release REQ

LLA RLC @ 00:07:22.650

BTS unit: 1:1
Channel No: 4 Name: DCCH
CFN: 242

Message Details:

#### CRLC AM Channel Release CNF

RLC LLA @ 00:07:22.650

BTS unit: 1:1
Channel No: 4 Name: DCCH
CFN: 242

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:07:22.660

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:3

#### CRLC_Config_REQ

RRC LLA @ 00:07:22.660

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:4

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC UM Channel Establish REQ

LLA RLC @ 00:07:22.670

BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 244

Message Details:

Configuration Parameters:

PU Size In Bits:136

#### CRLC UM Channel Establish CNF

RLC LLA @ 00:07:22.670

BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 244

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:07:22.680

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:4

#### CRLC_Config_REQ

RRC LLA @ 00:07:22.680

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:1

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode)

dl_UM_RLC_Mode:

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):136

dl_RLCModeInfo: (UL_RLC_Mode)

ul_UM_RLC_Mode:

transmissionRLC_Discard:

timerBasedNoExplicit (NoExplicitDiscard):dt100

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity):1
dLlogicalChannelIdentity (LogicalChannelIdentity):1
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC AM Channel Establish REQ

LLA RLC @ 00:07:22.680

BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 245

Message Details:

Configuration Parameters:

PU Size In Bits:128

Timer Parameters:

Poll (ms):200
Poll Prohibit (ms):0
EPC (ms):0
Discard (ms):0
Poll Periodic (ms):0
Status Prohibit (ms):0
Status Periodic (ms):0
Reset (ms):500
MRW (ms):0

Protocol Parameters:

Max Dat:15
Poll PU:0
Poll SDU:1
Poll Window:99
Max Reset:1
Tx Window Size:32
Rx Window Size:32
Max MRW:0
SDU Discard Mode:No discard

Polling Triggers:

Last PU In Buffer:On
Last PU In Retransmission Buffer:On
Poll Timer:On
Every Poll-PU PU:Off
Every Poll-SDU SDU:On
Poll-Window Percent Of Transmission Buffer:On
Timer Based:Off

Status Triggers:

Missing PU:On
Timer Based:Off
EPC Mechanism:Off

#### CRLC AM Channel Establish CNF

RLC LLA @ 00:07:22.690

BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 246

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:07:22.690

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:1

#### CRLC_Config_REQ

RRC LLA @ 00:07:22.690

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:2

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode)

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):128

dl_RLCModeInfo: (UL_RLC_Mode)

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity):2
dLlogicalChannelIdentity (LogicalChannelIdentity):2
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC AM Channel Establish REQ

LLA RLC @ 00:07:22.700

BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 247

Message Details:

Configuration Parameters:

PU Size In Bits:128

Timer Parameters:

Poll (ms):200
Poll Prohibit (ms):0
EPC (ms):0
Discard (ms):0
Poll Periodic (ms):0
Status Prohibit (ms):0
Status Periodic (ms):0
Reset (ms):500
MRW (ms):0

Protocol Parameters:

Max Dat:15
Poll PU:0
Poll SDU:1
Poll Window:99
Max Reset:1
Tx Window Size:32
Rx Window Size:32
Max MRW:0
SDU Discard Mode:No discard

Polling Triggers:

Last PU In Buffer:On
Last PU In Retransmission Buffer:On
Poll Timer:On
Every Poll-PU PU:Off
Every Poll-SDU SDU:On
Poll-Window Percent Of Transmission Buffer:On
Timer Based:Off

Status Triggers:

Missing PU:On
Timer Based:Off
EPC Mechanism:Off

#### CRLC AM Channel Establish CNF

RLC LLA @ 00:07:22.700

BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 247

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:07:22.710

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:2

#### CRLC_Config_REQ

RRC LLA @ 00:07:22.710

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:3

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode)

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):128

dl_RLCModeInfo: (UL_RLC_Mode)

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity):3
dLlogicalChannelIdentity (LogicalChannelIdentity):3
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC_Config_CNF

LLA RRC @ 00:07:22.720

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:3

#### CRLC_Config_REQ

RRC LLA @ 00:07:22.720

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:4

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode)

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):128

dl_RLCModeInfo: (UL_RLC_Mode)

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity):4
dLlogicalChannelIdentity (LogicalChannelIdentity):4
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC AM Channel Establish REQ

LLA RLC @ 00:07:22.720

BTS unit: 1:1
Channel No: 4 Name: DCCH
CFN: 249

Message Details:

Configuration Parameters:

PU Size In Bits:128

Timer Parameters:

Poll (ms):200
Poll Prohibit (ms):0
EPC (ms):0
Discard (ms):0
Poll Periodic (ms):0
Status Prohibit (ms):0
Status Periodic (ms):0
Reset (ms):500
MRW (ms):0

Protocol Parameters:

Max Dat:15
Poll PU:0
Poll SDU:1
Poll Window:99
Max Reset:1
Tx Window Size:32
Rx Window Size:32
Max MRW:0
SDU Discard Mode:No discard

Polling Triggers:

Last PU In Buffer:On
Last PU In Retransmission Buffer:On
Poll Timer:On
Every Poll-PU PU:Off
Every Poll-SDU SDU:On
Poll-Window Percent Of Transmission Buffer:On
Timer Based:Off

Status Triggers:

Missing PU:On
Timer Based:Off
EPC Mechanism:Off

#### CRLC AM Channel Establish CNF

RLC LLA @ 00:07:22.720

BTS unit: 1:1
Channel No: 4 Name: DCCH
CFN: 249

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:07:22.740

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:4

#### PHY_DATA_IND

PHY MAC @ 00:13:22.370

BTS unit: 1:1
Channel No: 0 Name: U_RACH
CFN: 98

Message Details:

TFI:0
TB set size:168
TB size:168
TB set (raw):

[0]08 44 48 8C D1 00 04 02
[8]00 02 C0 00 00 00 00 00
[16]00 00 00 00 00 00

TB set (decoded):

TB 0:

TCTF:0
MAC SDU (166 bits):

[0]21 11 22 33 44 00 10 08
[8]00 0B 00 00 00 00 00 00
[16]00 00 00 00 00

#### MAC_DATA_IND

MAC RLC @ 00:13:22.370

Category: Configuration
BTS unit: 1:1
Channel No: 0 Name: CCCH
CFN: 98

Message Details:

RLC PDU size (bits):166
RLC PDU (raw):

[0]21 11 22 33 44 00 10 08
[8]00 0B 00 00 00 00 00 00
[16]00 00 00 00 00

#### RLC_TR_DATA_IND: rrcConnectionRequest

RLC LLA @ 00:13:22.390

Channel No: 0 Name: CCCH

Message Details:

UL_CCCH_Message:

integrityCheckInfo: Omitted

message:

rrcConnectionRequest:

initialUE_Identity:

tmsi_and_LAI:

tmsi: 00010001001000100011001101000100

lai:

plmn_Identity:

mcc:

MCC.element: 0

MCC.element: 0

MCC.element: 1

mnc:

MNC.element: 0

MNC.element: 1

lac: 0000000000000001

establishmentCause: registration_EstablishmentCause [enum=12]

protocolErrorIndicator: noError_ProtocolErrorIndicator [enum=0]

measuredResultsOnRACH: Omitted

v3d0NonCriticalExtensions: Omitted

Layer 3 SDU:

[0]21 11 22 33 44 00 10 08
[8]00 0B 00 00 00 00 00 00
[16]00 00 00 00 00

#### RLC_TR_DATA_IND

LLA RRC @ 00:13:22.390

Channel ID: Rb0
Cell ID: 0

Message Details:

RLC_TR_DATA_IND:

cellId:0

routingInfo:

rB_Identity:0

tM_message:

uL_CCCH_Message:

integrityCheckInfo: Omit

message: (UL_CCCH_MessageType)

rrcConnectionRequest:

initialUE_Identity:

tmsi_and_LAI: (TMSI_and_LAI_GSM_MAP)

tmsi (TMSI_GSM_MAP):00010001001000100011001101000100

lai:

plmn_Identity:

mcc:

Digit:0
Digit:0
Digit:1

mnc:

Digit:0
Digit:1

lac:0000000000000001

establishmentCause:registration
protocolErrorIndicator:noError

measuredResultsOnRACH: Omit

v3d0NonCriticalExtensions: Omit

#### RLC_UM_DATA_REQ

RRC LLA @ 00:13:22.390

Channel ID: Rb0
Cell ID: 0

Message Details:

RLC_UM_DATA_REQ:

cellId:0

routingInfo:

rB_Identity:0

uM_message:

dL_CCCH_Message:

integrityCheckInfo: Omit

message: (DL_CCCH_MessageType)

rrcConnectionSetup:

r3:

rrcConnectionSetup_r3: (RRCConnectionSetup_r3_IEs)

initialUE_Identity:

tmsi_and_LAI: (TMSI_and_LAI_GSM_MAP)

tmsi (TMSI_GSM_MAP):00010001001000100011001101000100

lai:

plmn_Identity:

mcc:

Digit:0
Digit:0
Digit:1

mnc:

Digit:0
Digit:1

lac:0000000000000001

rrc_TransactionIdentifier:0
activationTime: Omit

new_U_RNTI: (U_RNTI)

srnc_Identity:000000000001
s_RNTI:00000000000000000001

new_c_RNTI (C_RNTI): Omit
rrc_StateIndicator:cell_DCH
utran_DRX_CycleLengthCoeff (UTRAN_DRX_CycleLengthCoefficient):9

capabilityUpdateRequirement:

ue_RadioCapabilityFDDUpdateRequirement:true
ue_RadioCapabilityTDDUpdateRequirement:false

systemSpecificCapUpdateReqList:

SystemSpecificCapUpdateReq:gsm

srb_InformationSetupList: (SRB_InformationSetupList2)

SRB_InformationSetup:

rb_Identity: Omit

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_UM_RLC_Mode:

transmissionRLC_Discard: Omit

dl_RLC_Mode:

dl_UM_RLC_Mode:

rb_MappingInfo:

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

dch (TransportChannelIdentity):5

logicalChannelIdentity:1

rlc_SizeList:

configured:

mac_LogicalChannelPriority:1

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

dch (TransportChannelIdentity):10

logicalChannelIdentity:1

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

rach:

logicalChannelIdentity:1

rlc_SizeList:

explicitList: (RLC_SizeExplicitList)

RLC_SizeInfo:

rlc_SizeIndex:1

mac_LogicalChannelPriority:1

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

fach:

logicalChannelIdentity:1

SRB_InformationSetup:

rb_Identity: Omit

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

rb_MappingInfo:

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

dch (TransportChannelIdentity):5

logicalChannelIdentity:2

rlc_SizeList:

configured:

mac_LogicalChannelPriority:2

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

dch (TransportChannelIdentity):10

logicalChannelIdentity:2

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

rach:

logicalChannelIdentity:2

rlc_SizeList:

explicitList: (RLC_SizeExplicitList)

RLC_SizeInfo:

rlc_SizeIndex:1

mac_LogicalChannelPriority:2

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

fach:

logicalChannelIdentity:2

SRB_InformationSetup:

rb_Identity: Omit

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

rb_MappingInfo:

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

dch (TransportChannelIdentity):5

logicalChannelIdentity:3

rlc_SizeList:

configured:

mac_LogicalChannelPriority:3

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

dch (TransportChannelIdentity):10

logicalChannelIdentity:3

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

rach:

logicalChannelIdentity:3

rlc_SizeList:

explicitList: (RLC_SizeExplicitList)

RLC_SizeInfo:

rlc_SizeIndex:1

mac_LogicalChannelPriority:3

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

fach:

logicalChannelIdentity:3

SRB_InformationSetup:

rb_Identity: Omit

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

rb_MappingInfo:

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

dch (TransportChannelIdentity):5

logicalChannelIdentity:4

rlc_SizeList:

configured:

mac_LogicalChannelPriority:4

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

dch (TransportChannelIdentity):10

logicalChannelIdentity:4

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

rach:

logicalChannelIdentity:4

rlc_SizeList:

explicitList: (RLC_SizeExplicitList)

RLC_SizeInfo:

rlc_SizeIndex:1

mac_LogicalChannelPriority:4

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

fach:

logicalChannelIdentity:4

ul_CommonTransChInfo:

tfc_Subset: Omit

prach_TFCS: (TFCS) Omit

modeSpecificInfo:

fdd:

ul_TFCS: (TFCS)

normalTFCI_Signalling: (ExplicitTFCS_Configuration)

complete: (TFCS_ReconfAdd)

ctfcSize:

ctfc2Bit:

:

ctfc2:0

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc2:1

powerOffsetInformation:

gainFactorInformation:

signalledGainFactors:

modeSpecificInfo:

fdd:

gainFactorBetaC (GainFactor):11

gainFactorBetaD (GainFactor):15
referenceTFC_ID:0

powerOffsetPp_m: Omit

ul_AddReconfTransChInfoList:

UL_AddReconfTransChInformation:

ul_TransportChannelType (UL_TrCH_Type):dch
transportChannelIdentity:5

transportFormatSet:

dedicatedTransChTFS:

tti:

tti10: (DedicatedDynamicTF_InfoList)

DedicatedDynamicTF_Info:

rlc_Size:

bitMode: (BitModeRLC_SizeInfo)

sizeType2:

part1:2
part2: Omit

numberOfTbSizeList:

NumberOfTransportBlocks:

zero:

NumberOfTransportBlocks:

one:

logicalChannelList:

allSizes:

semistaticTF_Information:

channelCodingType:

convolutional (CodingRate):third

rateMatchingAttribute:192
crc_Size:crc16

dl_CommonTransChInfo:

sccpch_TFCS: (TFCS) Omit

modeSpecificInfo:

fdd:

dl_Parameters:

sameAsUL:

dl_AddReconfTransChInfoList:

DL_AddReconfTransChInformation:

dl_TransportChannelType (DL_TrCH_Type):dch
dl_transportChannelIdentity (TransportChannelIdentity):10

tfs_SignallingMode:

sameAsULTrCH: (UL_TransportChannelIdentity)

ul_TransportChannelType (UL_TrCH_Type):dch
ul_TransportChannelIdentity (TransportChannelIdentity):5

dch_QualityTarget: (QualityTarget)

bler_QualityValue:-20

dummy: (TM_SignallingInfo) Omit

frequencyInfo: Omit

maxAllowedUL_TX_Power: Omit

ul_ChannelRequirement:

ul_DPCH_Info:

ul_DPCH_PowerControlInfo:

fdd:

dpcch_PowerOffset:-40
pc_Preamble:1
sRB_delay:7

powerControlAlgorithm:

algorithm1 (TPC_StepSizeFDD):0

modeSpecificInfo:

fdd:

scramblingCodeType:longSC
scramblingCode (UL_ScramblingCode):0
numberOfDPDCH: Omit
spreadingFactor:sf64
tfci_Existence:true
numberOfFBI_Bits: Omit
puncturingLimit:pl1

dl_CommonInformation:

dl_DPCH_InfoCommon:

cfnHandling:

initialise:

cfntargetsfnframeoffset: Omit

modeSpecificInfo:

fdd:

dl_DPCH_PowerControlInfo:

modeSpecificInfo:

fdd:

dpc_Mode:singleTPC

powerOffsetPilot_pdpdch:0

dl_rate_matching_restriction: Omit

spreadingFactorAndPilot: (SF512_AndPilot)

sfd128 (PilotBits128):pb4

positionFixedOrFlexible:fixed
tfci_Existence:false

modeSpecificInfo:

fdd:

defaultDPCH_OffsetValue (DefaultDPCH_OffsetValueFDD):0

dpch_CompressedModeInfo: Omit

tx_DiversityMode:noDiversity

ssdt_Information: Omit

dl_InformationPerRL_List:

DL_InformationPerRL:

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode:100

pdsch_SHO_DCH_Info: Omit

pdsch_CodeMapping: Omit

dl_DPCH_InfoPerRL:

fdd:

pCPICH_UsageForChannelEst:mayBeUsed
dpch_FrameOffset:0

secondaryCPICH_Info: Omit

dl_ChannelisationCodeList:

DL_ChannelisationCode:

secondaryScramblingCode:1

sf_AndCodeNumber: (SF512_AndCodeNumber)

sf128:0

scramblingCodeChange:noCodeChange

tpc_CombinationIndex:0
ssdt_CellIdentity: Omit
closedLoopTimingAdjMode: Omit

sccpch_InfoforFACH: Omit

laterNonCriticalExtensions: Omit

specialLI:true

#### RLC_UM_DATA_REQ: rrcConnectionSetup

LLA RLC @ 00:13:22.390

Channel No: 1 Name: CCCH

Message Details:

DL_CCCH_Message:

integrityCheckInfo: Omitted

message:

rrcConnectionSetup:

r3:

rrcConnectionSetup_r3:

initialUE_Identity:

tmsi_and_LAI:

tmsi: 00010001001000100011001101000100

lai:

plmn_Identity:

mcc:

MCC.element: 0

MCC.element: 0

MCC.element: 1

mnc:

MNC.element: 0

MNC.element: 1

lac: 0000000000000001

rrc_TransactionIdentifier: 0

activationTime: Omitted

new_U_RNTI:

srnc_Identity: 000000000001

s_RNTI: 00000000000000000001

new_c_RNTI: Omitted

rrc_StateIndicator: cell_DCH_RRC_StateIndicator [enum=0]

utran_DRX_CycleLengthCoeff: 9

capabilityUpdateRequirement:

ue_RadioCapabilityFDDUpdateRequirement: 1

ue_RadioCapabilityTDDUpdateRequirement: 0

systemSpecificCapUpdateReqList:

SystemSpecificCapUpdateReqList.element: gsm_SystemSpecificCapUpdateReq [enum=0]

srb_InformationSetupList:

SRB_InformationSetupList2.element:

rb_Identity: Omitted

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_UM_RLC_Mode:

transmissionRLC_Discard: Omitted

dl_RLC_Mode:

dl_UM_RLC_Mode: NULL

rb_MappingInfo:

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

dch: 5

logicalChannelIdentity: 1

rlc_SizeList:

configured: NULL

mac_LogicalChannelPriority: 1

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

dch: 10

logicalChannelIdentity: 1

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

rach: NULL

logicalChannelIdentity: 1

rlc_SizeList:

explicitList:

RLC_SizeExplicitList.element:

rlc_SizeIndex: 1

mac_LogicalChannelPriority: 1

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

fach: NULL

logicalChannelIdentity: 1

SRB_InformationSetupList2.element:

rb_Identity: Omitted

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard: dat15_MaxDAT [enum=10]

transmissionWindowSize: tw32_TransmissionWindowSize [enum=3]

timerRST: tr500_TimerRST [enum=9]

max_RST: rst1_MaxRST [enum=0]

pollingInfo:

timerPollProhibit: tpp200_TimerPollProhibit [enum=19]

timerPoll: tp200_TimerPoll [enum=19]

poll_PDU: Omitted

poll_SDU: sdu1_Poll_SDU [enum=0]

lastTransmissionPDU_Poll: 1

lastRetransmissionPDU_Poll: 1

pollWindow: pw99_PollWindow [enum=7]

timerPollPeriodic: Omitted

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery: 1

receivingWindowSize: rw32_ReceivingWindowSize [enum=3]

dl_RLC_StatusInfo:

timerStatusProhibit: tsp200_TimerStatusProhibit [enum=19]

timerEPC: Omitted

missingPDU_Indicator: 1

timerStatusPeriodic: Omitted

rb_MappingInfo:

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

dch: 5

logicalChannelIdentity: 2

rlc_SizeList:

configured: NULL

mac_LogicalChannelPriority: 2

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

dch: 10

logicalChannelIdentity: 2

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

rach: NULL

logicalChannelIdentity: 2

rlc_SizeList:

explicitList:

RLC_SizeExplicitList.element:

rlc_SizeIndex: 1

mac_LogicalChannelPriority: 2

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

fach: NULL

logicalChannelIdentity: 2

SRB_InformationSetupList2.element:

rb_Identity: Omitted

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard: dat15_MaxDAT [enum=10]

transmissionWindowSize: tw32_TransmissionWindowSize [enum=3]

timerRST: tr500_TimerRST [enum=9]

max_RST: rst1_MaxRST [enum=0]

pollingInfo:

timerPollProhibit: tpp200_TimerPollProhibit [enum=19]

timerPoll: tp200_TimerPoll [enum=19]

poll_PDU: Omitted

poll_SDU: sdu1_Poll_SDU [enum=0]

lastTransmissionPDU_Poll: 1

lastRetransmissionPDU_Poll: 1

pollWindow: pw99_PollWindow [enum=7]

timerPollPeriodic: Omitted

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery: 1

receivingWindowSize: rw32_ReceivingWindowSize [enum=3]

dl_RLC_StatusInfo:

timerStatusProhibit: tsp200_TimerStatusProhibit [enum=19]

timerEPC: Omitted

missingPDU_Indicator: 1

timerStatusPeriodic: Omitted

rb_MappingInfo:

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

dch: 5

logicalChannelIdentity: 3

rlc_SizeList:

configured: NULL

mac_LogicalChannelPriority: 3

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

dch: 10

logicalChannelIdentity: 3

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

rach: NULL

logicalChannelIdentity: 3

rlc_SizeList:

explicitList:

RLC_SizeExplicitList.element:

rlc_SizeIndex: 1

mac_LogicalChannelPriority: 3

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

fach: NULL

logicalChannelIdentity: 3

SRB_InformationSetupList2.element:

rb_Identity: Omitted

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard: dat15_MaxDAT [enum=10]

transmissionWindowSize: tw32_TransmissionWindowSize [enum=3]

timerRST: tr500_TimerRST [enum=9]

max_RST: rst1_MaxRST [enum=0]

pollingInfo:

timerPollProhibit: tpp200_TimerPollProhibit [enum=19]

timerPoll: tp200_TimerPoll [enum=19]

poll_PDU: Omitted

poll_SDU: sdu1_Poll_SDU [enum=0]

lastTransmissionPDU_Poll: 1

lastRetransmissionPDU_Poll: 1

pollWindow: pw99_PollWindow [enum=7]

timerPollPeriodic: Omitted

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery: 1

receivingWindowSize: rw32_ReceivingWindowSize [enum=3]

dl_RLC_StatusInfo:

timerStatusProhibit: tsp200_TimerStatusProhibit [enum=19]

timerEPC: Omitted

missingPDU_Indicator: 1

timerStatusPeriodic: Omitted

rb_MappingInfo:

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

dch: 5

logicalChannelIdentity: 4

rlc_SizeList:

configured: NULL

mac_LogicalChannelPriority: 4

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

dch: 10

logicalChannelIdentity: 4

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

rach: NULL

logicalChannelIdentity: 4

rlc_SizeList:

explicitList:

RLC_SizeExplicitList.element:

rlc_SizeIndex: 1

mac_LogicalChannelPriority: 4

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

fach: NULL

logicalChannelIdentity: 4

ul_CommonTransChInfo:

tfc_Subset: Omitted

prach_TFCS: Omitted

modeSpecificInfo:

fdd:

ul_TFCS:

normalTFCI_Signalling:

complete:

ctfcSize:

ctfc2Bit:

ctfc2Bit.noName:

ctfc2: 0

powerOffsetInformation:

gainFactorInformation:

computedGainFactors: 0

powerOffsetPp_m: Omitted

ctfc2Bit.noName:

ctfc2: 1

powerOffsetInformation:

gainFactorInformation:

signalledGainFactors:

modeSpecificInfo:

fdd:

gainFactorBetaC: 11

gainFactorBetaD: 15

referenceTFC_ID: 0

powerOffsetPp_m: Omitted

ul_AddReconfTransChInfoList:

UL_AddReconfTransChInfoList.element:

ul_TransportChannelType: dch_UL_TrCH_Type [enum=0]

transportChannelIdentity: 5

transportFormatSet:

dedicatedTransChTFS:

tti:

tti10:

DedicatedDynamicTF_InfoList.element:

rlc_Size:

bitMode:

sizeType2:

part1: 2

part2: Omitted

numberOfTbSizeList:

numberOfTbSizeList.element:

zero: NULL

numberOfTbSizeList.element:

one: NULL

logicalChannelList:

allSizes: NULL

semistaticTF_Information:

channelCodingType:

convolutional: third_CodingRate [enum=1]

rateMatchingAttribute: 192

crc_Size: crc16_CRC_Size [enum=3]

dl_CommonTransChInfo:

sccpch_TFCS: Omitted

modeSpecificInfo:

fdd:

dl_Parameters:

sameAsUL: NULL

dl_AddReconfTransChInfoList:

DL_AddReconfTransChInfoList.element:

dl_TransportChannelType: dch_DL_TrCH_Type [enum=0]

dl_transportChannelIdentity: 10

tfs_SignallingMode:

sameAsULTrCH:

ul_TransportChannelType: dch_UL_TrCH_Type [enum=0]

ul_TransportChannelIdentity: 5

dch_QualityTarget:

bler_QualityValue: -20

dummy: Omitted

frequencyInfo: Omitted

maxAllowedUL_TX_Power: Omitted

ul_ChannelRequirement:

ul_DPCH_Info:

ul_DPCH_PowerControlInfo:

fdd:

dpcch_PowerOffset: -40

pc_Preamble: 1

sRB_delay: 7

powerControlAlgorithm:

algorithm1: 0

modeSpecificInfo:

fdd:

scramblingCodeType: longSC_ScramblingCodeType [enum=1]

scramblingCode: 0

numberOfDPDCH: Default

spreadingFactor: sf64_SpreadingFactor [enum=4]

tfci_Existence: 1

numberOfFBI_Bits: Omitted

puncturingLimit: pl1_PuncturingLimit [enum=15]

dl_CommonInformation:

dl_DPCH_InfoCommon:

cfnHandling:

initialise:

cfntargetsfnframeoffset: Omitted

modeSpecificInfo:

fdd:

dl_DPCH_PowerControlInfo:

modeSpecificInfo:

fdd:

dpc_Mode: singleTPC_DPC_Mode [enum=0]

powerOffsetPilot_pdpdch: 0

dl_rate_matching_restriction: Omitted

spreadingFactorAndPilot:

sfd128: pb4_PilotBits128 [enum=0]

positionFixedOrFlexible: fixed_PositionFixedOrFlexible [enum=0]

tfci_Existence: 0

modeSpecificInfo:

fdd:

defaultDPCH_OffsetValue: 0

dpch_CompressedModeInfo: Omitted

tx_DiversityMode: noDiversity_TX_DiversityMode [enum=0]

ssdt_Information: Omitted

dl_InformationPerRL_List:

DL_InformationPerRL_List.element:

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode: 100

pdsch_SHO_DCH_Info: Omitted

pdsch_CodeMapping: Omitted

dl_DPCH_InfoPerRL:

fdd:

pCPICH_UsageForChannelEst: mayBeUsed_PCPICH_UsageForChannelEst [enum=0]

dpch_FrameOffset: 0

secondaryCPICH_Info: Omitted

dl_ChannelisationCodeList:

DL_ChannelisationCodeList.element:

secondaryScramblingCode: 1

sf_AndCodeNumber:

sf128: 0

scramblingCodeChange: noCodeChange_ScramblingCodeChange [enum=1]

tpc_CombinationIndex: 0

ssdt_CellIdentity: Omitted

closedLoopTimingAdjMode: Omitted

sccpch_InfoforFACH: Omitted

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]30 E7 22 24 46 68 80 02
[8]01 00 01 00 04 00 00 4D
[16]82 69 3A 10 10 89 0D 42
[24]00 02 81 9E 8E 46 C9 A6
[32]7C 9C 4E 74 20 A5 12 3A
[40]8C 00 15 13 3D 1C 8D 93
[48]4C F9 38 9C E8 42 52 24
[56]B5 28 00 4A 46 7A 39 1B
[64]26 99 F2 71 39 D0 86 B4
[72]49 EA 70 00 D4 C8 00 06
[80]25 2B F0 02 00 08 82 23
[88]BF 66 08 98 95 A5 47 82
[96]00 00 01 3F 90 0A 14 00
[104]02 06 40 00 0C 28 08

#### MAC_DATA_REQ

RLC MAC @ 00:13:22.430

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: CCCH
CFN: 124

Message Details:

RLC PDU size (bits):160
RLC PDU (raw):

[0]31 F8 30 E7 22 24 46 68
[8]80 02 01 00 01 00 04 00
[16]00 4D 82 69

RLC PDU (decoded):

Sequence number:24
Length indicator 0 (octets):124 (the first data octet in this RLC PDU is the first octet of a RLC SDU)
Segment associated with length indicator 0 (0 octets):

Last segment, not associated with any length indicators (18 octets):

[0]30 E7 22 24 46 68 80 02
[8]01 00 01 00 04 00 00 4D
[16]82 69

#### MAC_DATA_REQ

RLC MAC @ 00:13:22.430

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: CCCH
CFN: 124

Message Details:

RLC PDU size (bits):160
RLC PDU (raw):

[0]32 3A 10 10 89 0D 42 00
[8]02 81 9E 8E 46 C9 A6 7C
[16]9C 4E 74 20

RLC PDU (decoded):

Sequence number:25
Last segment, not associated with any length indicators (19 octets):

[0]3A 10 10 89 0D 42 00 02
[8]81 9E 8E 46 C9 A6 7C 9C
[16]4E 74 20

#### MAC_DATA_REQ

RLC MAC @ 00:13:22.430

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: CCCH
CFN: 124

Message Details:

RLC PDU size (bits):160
RLC PDU (raw):

[0]34 A5 12 3A 8C 00 15 13
[8]3D 1C 8D 93 4C F9 38 9C
[16]E8 42 52 24

RLC PDU (decoded):

Sequence number:26
Last segment, not associated with any length indicators (19 octets):

[0]A5 12 3A 8C 00 15 13 3D
[8]1C 8D 93 4C F9 38 9C E8
[16]42 52 24

#### MAC_DATA_REQ

RLC MAC @ 00:13:22.430

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: CCCH
CFN: 124

Message Details:

RLC PDU size (bits):160
RLC PDU (raw):

[0]36 B5 28 00 4A 46 7A 39
[8]1B 26 99 F2 71 39 D0 86
[16]B4 49 EA 70

RLC PDU (decoded):

Sequence number:27
Last segment, not associated with any length indicators (19 octets):

[0]B5 28 00 4A 46 7A 39 1B
[8]26 99 F2 71 39 D0 86 B4
[16]49 EA 70

#### MAC_DATA_REQ

RLC MAC @ 00:13:22.430

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: CCCH
CFN: 124

Message Details:

RLC PDU size (bits):160
RLC PDU (raw):

[0]38 00 D4 C8 00 06 25 2B
[8]F0 02 00 08 82 23 BF 66
[16]08 98 95 A5

RLC PDU (decoded):

Sequence number:28
Last segment, not associated with any length indicators (19 octets):

[0]00 D4 C8 00 06 25 2B F0
[8]02 00 08 82 23 BF 66 08
[16]98 95 A5

#### MAC_DATA_REQ

RLC MAC @ 00:13:22.430

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: CCCH
CFN: 124

Message Details:

RLC PDU size (bits):160
RLC PDU (raw):

[0]3B 23 FE 47 82 00 00 01
[8]3F 90 0A 14 00 02 06 40
[16]00 0C 28 08

RLC PDU (decoded):

Sequence number:29
Length indicator 0 (octets):17
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (17 octets):

[0]47 82 00 00 01 3F 90 0A
[8]14 00 02 06 40 00 0C 28
[16]08
Padding associated with length indicator 1 (0 octets):

#### PHY_DATA_REQ

MAC PHY @ 00:13:22.430

BTS unit: 1:1
Channel No: 0 Name: FACH
CFN: 124

Message Details:

TFI:2
TB set size:336
TB size:168
TB set (raw, each TB word aligned):

[0]40 31 F8 30 E7 22 24 46
[8]68 80 02 01 00 01 00 04
[16]00 00 4D 82 69 00 40 32
[24]3A 10 10 89 0D 42 00 02
[32]81 9E 8E 46 C9 A6 7C 9C
[40]4E 74 20 00

TB set (decoded):

TB 0:

TCTF:64
MAC SDU (160 bits):

[0]31 F8 30 E7 22 24 46 68
[8]80 02 01 00 01 00 04 00
[16]00 4D 82 69

TB 1:

TCTF:64
MAC SDU (160 bits):

[0]32 3A 10 10 89 0D 42 00
[8]02 81 9E 8E 46 C9 A6 7C
[16]9C 4E 74 20

#### PHY_DATA_REQ

MAC PHY @ 00:13:22.440

BTS unit: 1:1
Channel No: 0 Name: FACH
CFN: 125

Message Details:

TFI:2
TB set size:336
TB size:168
TB set (raw, each TB word aligned):

[0]40 34 A5 12 3A 8C 00 15
[8]13 3D 1C 8D 93 4C F9 38
[16]9C E8 42 52 24 00 40 36
[24]B5 28 00 4A 46 7A 39 1B
[32]26 99 F2 71 39 D0 86 B4
[40]49 EA 70 00

TB set (decoded):

TB 0:

TCTF:64
MAC SDU (160 bits):

[0]34 A5 12 3A 8C 00 15 13
[8]3D 1C 8D 93 4C F9 38 9C
[16]E8 42 52 24

TB 1:

TCTF:64
MAC SDU (160 bits):

[0]36 B5 28 00 4A 46 7A 39
[8]1B 26 99 F2 71 39 D0 86
[16]B4 49 EA 70

#### PHY_DATA_REQ

MAC PHY @ 00:13:22.450

BTS unit: 1:1
Channel No: 0 Name: FACH
CFN: 126

Message Details:

TFI:2
TB set size:336
TB size:168
TB set (raw, each TB word aligned):

[0]40 38 00 D4 C8 00 06 25
[8]2B F0 02 00 08 82 23 BF
[16]66 08 98 95 A5 00 40 3B
[24]23 FE 47 82 00 00 01 3F
[32]90 0A 14 00 02 06 40 00
[40]0C 28 08 00

TB set (decoded):

TB 0:

TCTF:64
MAC SDU (160 bits):

[0]38 00 D4 C8 00 06 25 2B
[8]F0 02 00 08 82 23 BF 66
[16]08 98 95 A5

TB 1:

TCTF:64
MAC SDU (160 bits):

[0]3B 23 FE 47 82 00 00 01
[8]3F 90 0A 14 00 02 06 40
[16]00 0C 28 08

#### CPHY_SYNC_IND

PHY RRC @ 00:13:22.670

BTS unit: 1:1
Channel No: 0 Name: U_DPCH
CFN: 148

Message Details:

#### PHY_DATA_IND

PHY MAC @ 00:13:22.830

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 144

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 00 04 B0 C0 00 08 00
[8]00 51 1B 8D D0 6A 4C 66
[16]88 A2 C0 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 00 4B 0C 00 00 80 00
[8]05 11 B8 DD 06 A4 C6 68
[16]8A 2C

#### MAC_DATA_IND

MAC RLC @ 00:13:22.830

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 144

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 00 4B 0C 00 00 80 00
[8]05 11 B8 DD 06 A4 C6 68
[16]8A 2C

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:0
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]4B 0C 00 00 80 00 05 11
[8]B8 DD 06 A4 C6 68 8A 2C

#### PHY_DATA_IND

PHY MAC @ 00:13:22.840

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 145

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 00 88 30 34 80 01 80
[8]01 18 FC FC 0C C0 D5 C6
[16]28 48 C0 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 08 83 03 48 00 18 00
[8]11 8F CF C0 CC 0D 5C 62
[16]84 8C

#### MAC_DATA_IND

MAC RLC @ 00:13:22.840

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 145

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 08 83 03 48 00 18 00
[8]11 8F CF C0 CC 0D 5C 62
[16]84 8C

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:1
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]83 03 48 00 18 00 11 8F
[8]CF C0 CC 0D 5C 62 84 8C

#### PHY_DATA_IND

PHY MAC @ 00:13:22.850

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 146

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 01 50 BF E0 28 99 01
[8]00 05 55 55 55 55 55 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 15 0B FE 02 89 90 10
[8]00 55 55 55 55 55 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:13:22.850

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 146

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 15 0B FE 02 89 90 10
[8]00 55 55 55 55 55 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:2
Polling bit:1 (request a status report)
Length indicator 0 (octets):5
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (5 octets):

[0]02 89 90 10 00
Padding associated with length indicator 1 (9 octets):

[0]55 55 55 55 55 55 55 55
[8]55

#### MAC_DATA_REQ

RLC MAC @ 00:13:22.860

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 167

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:3

#### PHY_DATA_REQ

MAC PHY @ 00:13:22.860

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 167

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]10 20 03 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:13:22.860

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 147

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 00 01 50 08 80 09 82
[8]84 38 80 78 88 00 00 AB
[16]82 FA 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 00 15 00 88 00 98 28
[8]43 88 07 88 80 00 0A B8
[16]2F A0

#### MAC_DATA_IND

MAC RLC @ 00:13:22.860

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 147

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 00 15 00 88 00 98 28
[8]43 88 07 88 80 00 0A B8
[16]2F A0

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:0
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]15 00 88 00 98 28 43 88
[8]07 88 80 00 0A B8 2F A0

#### PHY_DATA_IND

PHY MAC @ 00:13:22.870

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 148

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 00 D1 9F E8 91 19 A2
[8]19 81 AB 8C 50 A0 00 04
[16]05 55 50 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 0D 19 FE 89 11 9A 21
[8]98 1A B8 C5 0A 00 00 40
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:13:22.870

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 148

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 0D 19 FE 89 11 9A 21
[8]98 1A B8 C5 0A 00 00 40
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:1
Polling bit:1 (request a status report)
Length indicator 0 (octets):12
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (12 octets):

[0]89 11 9A 21 98 1A B8 C5
[8]0A 00 00 40
Padding associated with length indicator 1 (2 octets):

[0]55 55

#### MAC_DATA_REQ

RLC MAC @ 00:13:22.880

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 169

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 20 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:2

#### PHY_DATA_REQ

MAC PHY @ 00:13:22.880

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 169

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 02 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 20 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### RLC_AM_DATA_IND: rrcConnectionSetupComplete

RLC LLA @ 00:13:22.890

Channel No: 2 Name: DCCH

Message Details:

UL_DCCH_Message:

integrityCheckInfo: Omitted

message:

rrcConnectionSetupComplete:

rrc_TransactionIdentifier: 0

startList:

STARTList.element:

cn_DomainIdentity: ps_domain_CN_DomainIdentity [enum=1]

start_Value: 00000000000000000010

STARTList.element:

cn_DomainIdentity: cs_domain_CN_DomainIdentity [enum=0]

start_Value: 00000000000000000010

ue_RadioAccessCapability:

accessStratumReleaseIndicator: r99_AccessStratumReleaseIndicator [enum=0]

pdcp_Capability:

losslessSRNS_RelocationSupport: 0

supportForRfc2507:

notSupported: NULL

rlc_Capability:

totalRLC_AM_BufferSize: kb50_TotalRLC_AM_BufferSize [enum=2]

maximumRLC_WindowSize: mws2047_MaximumRLC_WindowSize [enum=0]

maximumAM_EntityNumber: am6_MaximumAM_EntityNumberRLC_Cap [enum=3]

transportChannelCapability:

dl_TransChCapability:

maxNoBitsReceived: b8960_MaxNoBits [enum=7]

maxConvCodeBitsReceived: b1280_MaxNoBits [enum=1]

turboDecodingSupport:

supported: b8960_MaxNoBits [enum=7]

maxSimultaneousTransChs: e8_MaxSimultaneousTransChsDL [enum=1]

maxSimultaneousCCTrCH_Count: 1

maxReceivedTransportBlocks: tb32_MaxTransportBlocksDL [enum=3]

maxNumberOfTFC: tfc128_MaxNumberOfTFC_DL [enum=5]

maxNumberOfTF: tf64_MaxNumberOfTF [enum=1]

ul_TransChCapability:

maxNoBitsTransmitted: b3840_MaxNoBits [enum=3]

maxConvCodeBitsTransmitted: b1280_MaxNoBits [enum=1]

turboEncodingSupport:

supported: b3840_MaxNoBits [enum=3]

maxSimultaneousTransChs: e8_MaxSimultaneousTransChsUL [enum=2]

modeSpecificInfo:

fdd: NULL

maxTransmittedBlocks: tb32_MaxTransportBlocksUL [enum=4]

maxNumberOfTFC: tfc64_MaxNumberOfTFC_UL [enum=5]

maxNumberOfTF: tf32_MaxNumberOfTF [enum=0]

rf_Capability:

fddRF_Capability:

ue_PowerClass: 4

txRxFrequencySeparation: mhz190_TxRxFrequencySeparation [enum=0]

tddRF_Capability: Omitted

physicalChannelCapability:

fddPhysChCapability:

downlinkPhysChCapability:

maxNoDPCH_PDSCH_Codes: 1

maxNoPhysChBitsReceived: b9600_MaxNoPhysChBitsReceived [enum=6]

supportForSF_512: 0

supportOfPDSCH: 0

simultaneousSCCPCH_DPCH_Reception:

notSupported: NULL

uplinkPhysChCapability:

maxNoDPDCH_BitsTransmitted: b4800_MaxNoDPDCH_BitsTransmitted [enum=3]

supportOfPCPCH: 0

tddPhysChCapability: Omitted

ue_MultiModeRAT_Capability:

multiRAT_CapabilityList:

supportOfGSM: 1

supportOfMulticarrier: 0

multiModeCapability: fdd_MultiModeCapability [enum=1]

securityCapability:

cipheringAlgorithmCap: 0000000000000011

integrityProtectionAlgorithmCap: 0000000000000010

ue_positioning_Capability:

standaloneLocMethodsSupported: 0

ue_BasedOTDOA_Supported: 0

networkAssistedGPS_Supported: noNetworkAssistedGPS_NetworkAssistedGPS_Supported [enum=3]

supportForUE_GPS_TimingOfCellFrames: 0

supportForIPDL: 0

measurementCapability:

downlinkCompressedMode:

fdd_Measurements: 1

tdd_Measurements: Omitted

gsm_Measurements:

gsm900: 1

dcs1800: 1

gsm1900: 1

multiCarrierMeasurements: 0

uplinkCompressedMode:

fdd_Measurements: 1

tdd_Measurements: Omitted

gsm_Measurements:

gsm900: 1

dcs1800: 1

gsm1900: 1

multiCarrierMeasurements: 0

ue_RATSpecificCapability:

InterRAT_UE_RadioAccessCapabilityList.element:

gsm:

gsm_Classmark2: 33035718A1

gsm_Classmark3: 60144C8080

v370NonCriticalExtensions: Omitted

Layer 3 SDU:

[0]4B 0C 00 00 80 00 05 11
[8]B8 DD 06 A4 C6 68 8A 2C
[16]83 03 48 00 18 00 11 8F
[24]CF C0 CC 0D 5C 62 84 8C
[32]02 89 90 10 00

#### RLC_AM_DATA_IND

LLA RRC @ 00:13:22.890

Channel ID: Rb2
Cell ID: -1

Message Details:

RLC_AM_DATA_IND:

cellId:-1

routingInfo:

rB_Identity:2

integrityResult:

integrityUsed (IntegrityStatus):i_pass

aM_message:

uL_DCCH_Message:

integrityCheckInfo: Omit

message: (UL_DCCH_MessageType)

rrcConnectionSetupComplete:

rrc_TransactionIdentifier:0

startList:

STARTSingle:

cn_DomainIdentity:ps_domain
start_Value:00000000000000000010

STARTSingle:

cn_DomainIdentity:cs_domain
start_Value:00000000000000000010

ue_RadioAccessCapability:

accessStratumReleaseIndicator:r99

pdcp_Capability:

losslessSRNS_RelocationSupport:false

supportForRfc2507:

notSupported:

rlc_Capability:

totalRLC_AM_BufferSize:kb50
maximumRLC_WindowSize:mws2047
maximumAM_EntityNumber (MaximumAM_EntityNumberRLC_Cap):am6

transportChannelCapability:

dl_TransChCapability:

maxNoBitsReceived (MaxNoBits):b8960
maxConvCodeBitsReceived (MaxNoBits):b1280

turboDecodingSupport: (TurboSupport)

supported (MaxNoBits):b8960

maxSimultaneousTransChs (MaxSimultaneousTransChsDL):e8
maxSimultaneousCCTrCH_Count:1
maxReceivedTransportBlocks (MaxTransportBlocksDL):tb32
maxNumberOfTFC (MaxNumberOfTFC_DL):tfc128
maxNumberOfTF:tf64

ul_TransChCapability:

maxNoBitsTransmitted (MaxNoBits):b3840
maxConvCodeBitsTransmitted (MaxNoBits):b1280

turboEncodingSupport: (TurboSupport)

supported (MaxNoBits):b3840

maxSimultaneousTransChs (MaxSimultaneousTransChsUL):e8

modeSpecificInfo:

fdd:

maxTransmittedBlocks (MaxTransportBlocksUL):tb32
maxNumberOfTFC (MaxNumberOfTFC_UL):tfc64
maxNumberOfTF:tf32

rf_Capability:

fddRF_Capability:

ue_PowerClass:4
txRxFrequencySeparation:mhz190

tddRF_Capability: Omit

physicalChannelCapability:

fddPhysChCapability:

downlinkPhysChCapability: (DL_PhysChCapabilityFDD)

maxNoDPCH_PDSCH_Codes:1
maxNoPhysChBitsReceived:b9600
supportForSF_512:false
supportOfPDSCH:false

simultaneousSCCPCH_DPCH_Reception:

notSupported:

uplinkPhysChCapability: (UL_PhysChCapabilityFDD)

maxNoDPDCH_BitsTransmitted:b4800
supportOfPCPCH:false

tddPhysChCapability: Omit

ue_MultiModeRAT_Capability:

multiRAT_CapabilityList: (MultiRAT_Capability)

supportOfGSM:true
supportOfMulticarrier:false

multiModeCapability:fdd

securityCapability:

cipheringAlgorithmCap:0000000000000011
integrityProtectionAlgorithmCap:0000000000000010

ue_positioning_Capability:

standaloneLocMethodsSupported:false
ue_BasedOTDOA_Supported:false
networkAssistedGPS_Supported:noNetworkAssistedGPS
supportForUE_GPS_TimingOfCellFrames:false
supportForIPDL:false

measurementCapability:

downlinkCompressedMode: (CompressedModeMeasCapability)

fdd_Measurements:true
tdd_Measurements: Omit

gsm_Measurements:

gsm900:true
dcs1800:true
gsm1900:true

multiCarrierMeasurements:false

uplinkCompressedMode: (CompressedModeMeasCapability)

fdd_Measurements:true
tdd_Measurements: Omit

gsm_Measurements:

gsm900:true
dcs1800:true
gsm1900:true

multiCarrierMeasurements:false

ue_RATSpecificCapability: (InterRAT_UE_RadioAccessCapabilityList)

InterRAT_UE_RadioAccessCapability:

gsm:

gsm_Classmark2:

[0]33 03 57 18 A1
gsm_Classmark3:

[0]60 14 4C 80 80

v370NonCriticalExtensions: Omit

#### RLC_AM_DATA_IND: initialDirectTransfer

RLC RRC @ 00:13:22.880

Channel No: 3 Name: DCCH

Message Details:

UL_DCCH_Message:

integrityCheckInfo: Omitted

message:

initialDirectTransfer:

cn_DomainIdentity: cs_domain_CN_DomainIdentity [enum=0]

intraDomainNasNodeSelector:

version:

release99:

cn_Type:

gsm_Map_IDNNS:

routingbasis:

localPTMSI:

routingparameter: 0010001000

enteredparameter: 0

nas_Message: 05087100F11000015705F41122334433035718A1

measuredResultsOnRACH: Omitted

v3a0NonCriticalExtensions:

initialDirectTransfer_v3a0ext:

start_Value: 00000000000000000010

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]15 00 88 00 98 28 43 88
[8]07 88 80 00 0A B8 2F A0
[16]89 11 9A 21 98 1A B8 C5
[24]0A 00 00 40

#### RRC_DATA_IND: mm:locationUpdatingRequest

RRC NAS @ 00:13:22.880

Cell ID: -1

Message Details:

LOCATIONUPDATINGREQUEST:

skipIndicator: 0000

mMProtocolDiscriminator: 0101

msgType: 00001000

ciphKeySeqNum:

spare1: 0

keySeq: 111

locUpdType:

fOR: 0

spare1: 0

lUT: 01

locAreaId:

plmn: 00F110

lac: 0001

mSClsmk1:

spare1: 0

revLvl: 10

eSIND: 1

a5_1: 0

rFPwrCap: 111

mobileId:

iel: 05

iDigit1: 1111

oddEvenInd: 0

typeOfId: 100

otherDigits: 11223344

mSClsmk2:

iei: 00110011

iel: 03

spare1_1: 0

revLvl: 10

eSIND: 1

a5_1: 0

rFPwrCap: 111

spare1_2: 0

pSCap: 0

sSSI: 01

sMCap: 1

vBS: 0

vGCS: 0

fC: 0

cM3: 1

spare1_3: 0

lCSVA: 1

uCS2: 0

soLSA: 0

cMSP: 0

a5_3: 0

a5_2: 1

#### RRC_DATA_REQ: mm:authenticationRequest

NAS RRC @ 00:13:22.910

Cell ID: -1

Message Details:

AUTHENTICATIONREQUEST:

skipIndicator: 0000

mMProtocolDiscriminator: 0101

msgType: 00010010

spare4: 0000

ciphKeySeqNum:

spare1: 0

keySeq: 000

rAND: 01010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101

aUTN:

iei: 00100000

iel: 10

aUTN: 01100110000100010000000000110011001000101101110100000000000000000101010101000100011101110110011000010001000000000011001100100010

#### RLC_AM_DATA_REQ:downlinkDirectTransfer

RRC RLC @ 00:13:22.910

Channel No: 3 Name: DCCH

Message Details:

Opt1: 0

Opt2: 0

DL_DCCH_Message:

integrityCheckInfo: Omitted

message:

downlinkDirectTransfer:

r3:

downlinkDirectTransfer_r3:

rrc_TransactionIdentifier: 0

cn_DomainIdentity: cs_domain_CN_DomainIdentity [enum=0]

nas_Message: 0512005555555555555555555555555555555520106611003322DD00005544776611003322

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]14 00 48 0A 24 00 AA AA
[8]AA AA AA AA AA AA AA AA
[16]AA AA AA AA AA AA 40 20
[24]CC 22 00 66 45 BA 00 00
[32]AA 88 EE CC 22 00 66 44

#### MAC_DATA_REQ

RLC MAC @ 00:13:22.920

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 173

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 00 14 00 48 0A 24 00
[8]AA AA AA AA AA AA AA AA
[16]AA AA

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:0
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]14 00 48 0A 24 00 AA AA
[8]AA AA AA AA AA AA AA AA

#### MAC_DATA_REQ

RLC MAC @ 00:13:22.920

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 173

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 08 AA AA AA AA AA AA
[8]40 20 CC 22 00 66 45 BA
[16]00 00

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:1
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]AA AA AA AA AA AA 40 20
[8]CC 22 00 66 45 BA 00 00

#### MAC_DATA_REQ

RLC MAC @ 00:13:22.920

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 173

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 15 11 FE AA 88 EE CC
[8]22 00 66 44 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:2
Polling bit:1 (request a status report)
Length indicator 0 (octets):8
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (8 octets):

[0]AA 88 EE CC 22 00 66 44
Padding associated with length indicator 1 (6 octets):

[0]00 00 00 00 00 00

#### PHY_DATA_REQ

MAC PHY @ 00:13:22.920

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 173

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 00 01 40 04 80 A2 40
[8]0A AA AA AA AA AA AA AA
[16]AA AA A0 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 00 14 00 48 0A 24 00
[8]AA AA AA AA AA AA AA AA
[16]AA AA

#### PHY_DATA_REQ

MAC PHY @ 00:13:22.930

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 174

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 00 8A AA AA AA AA AA
[8]A4 02 0C C2 20 06 64 5B
[16]A0 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 08 AA AA AA AA AA AA
[8]40 20 CC 22 00 66 45 BA
[16]00 00

#### PHY_DATA_REQ

MAC PHY @ 00:13:22.940

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 175

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 01 51 1F EA A8 8E EC
[8]C2 20 06 64 40 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 15 11 FE AA 88 EE CC
[8]22 00 66 44 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:13:23.060

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 167

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 01 50 BF E0 28 99 01
[8]00 05 55 55 55 55 55 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 15 0B FE 02 89 90 10
[8]00 55 55 55 55 55 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:13:23.060

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 167

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 15 0B FE 02 89 90 10
[8]00 55 55 55 55 55 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:2
Polling bit:1 (request a status report)
Length indicator 0 (octets):5
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (5 octets):

[0]02 89 90 10 00
Padding associated with length indicator 1 (9 octets):

[0]55 55 55 55 55 55 55 55
[8]55

#### MAC_DATA_REQ

RLC MAC @ 00:13:23.070

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 188

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:3

#### PHY_DATA_REQ

MAC PHY @ 00:13:23.070

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 188

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]10 20 03 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:13:23.080

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 169

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 00 D1 9F E8 91 19 A2
[8]19 81 AB 8C 50 A0 00 04
[16]05 55 50 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 0D 19 FE 89 11 9A 21
[8]98 1A B8 C5 0A 00 00 40
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:13:23.080

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 169

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 0D 19 FE 89 11 9A 21
[8]98 1A B8 C5 0A 00 00 40
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:1
Polling bit:1 (request a status report)
Length indicator 0 (octets):12
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (12 octets):

[0]89 11 9A 21 98 1A B8 C5
[8]0A 00 00 40
Padding associated with length indicator 1 (2 octets):

[0]55 55

#### MAC_DATA_REQ

RLC MAC @ 00:13:23.090

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 190

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 20 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:2

#### PHY_DATA_REQ

MAC PHY @ 00:13:23.090

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 190

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 02 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 20 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### MAC_DATA_REQ

RLC MAC @ 00:13:23.120

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 193

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 15 11 FE AA 88 EE CC
[8]22 00 66 44 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:2
Polling bit:1 (request a status report)
Length indicator 0 (octets):8
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (8 octets):

[0]AA 88 EE CC 22 00 66 44
Padding associated with length indicator 1 (6 octets):

[0]00 00 00 00 00 00

#### PHY_DATA_REQ

MAC PHY @ 00:13:23.120

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 193

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 01 51 1F EA A8 8E EC
[8]C2 20 06 64 40 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 15 11 FE AA 88 EE CC
[8]22 00 66 44 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:13:23.170

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 178

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 03 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### MAC_DATA_IND

MAC RLC @ 00:13:23.170

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 178

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:3

#### PHY_DATA_IND

PHY MAC @ 00:13:23.320

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 193

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 01 51 E6 C0 05 82 AA
[8]2A A2 3B B3 10 82 08 80
[16]19 91 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 15 1E 6C 00 58 2A A2
[8]AA 23 BB 31 08 20 88 01
[16]99 10

#### MAC_DATA_IND

MAC RLC @ 00:13:23.320

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 193

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 15 1E 6C 00 58 2A A2
[8]AA 23 BB 31 08 20 88 01
[16]99 10

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:2
Polling bit:1 (request a status report)
Length indicator 0 (octets):15
Segment associated with length indicator 0 (15 octets):

[0]6C 00 58 2A A2 AA 23 BB
[8]31 08 20 88 01 99 10

#### RLC_AM_DATA_IND: uplinkDirectTransfer

RLC RRC @ 00:13:23.330

Channel No: 3 Name: DCCH

Message Details:

UL_DCCH_Message:

integrityCheckInfo: Omitted

message:

uplinkDirectTransfer:

cn_DomainIdentity: cs_domain_CN_DomainIdentity [enum=0]

nas_Message: 055455447766210411003322

measuredResultsOnRACH: Omitted

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]6C 00 58 2A A2 AA 23 BB
[8]31 08 20 88 01 99 10

#### RRC_DATA_IND: mm:authenticationResponse

RRC NAS @ 00:13:23.330

Cell ID: -1

Message Details:

AUTHENTICATIONRESPONSE:

skipIndicator: 0000

mMProtocolDiscriminator: 0101

msgType: 01010100

authRsp: 01010101010001000111011101100110

authRspExt:

iei: 00100001

iel: 04

rES: 00010001000000000011001100100010

#### MAC_DATA_REQ

RLC MAC @ 00:13:23.330

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 214

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:3

#### PHY_DATA_REQ

MAC PHY @ 00:13:23.330

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 214

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 03 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### CRLC_SecurityMode_Config_REQ

RRC LLA @ 00:13:23.350

Cell ID: -1

Message Details:

CRLC_SecurityMode_Config_REQ:

cellId:-1

rlcSecurityInfo: (SecurityInfo)

cn_DomainIdentity:cs_domain
startValue (START_Value):00000000000000000000
cipheringKey: Omit
integrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
gsmCipheringKey: Omit

#### CRLC_SecurityMode_Config_REQ

RRC RLC @ 00:13:23.350

Message Details:

cellIdentity: 1

rlcSecurityInfo:

cn_DomainIdentity: cs_domain_CN_DomainIdentity

startValue: 00000000000000000000

cipheringKey: Omitted

integrityKey: 01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100

#### CRLC_SecurityMode_Config_CNF

LLA RRC @ 00:13:23.360

Cell ID: -1

Message Details:

CRLC_SecurityMode_Config_CNF:

cellId:-1

#### CRLC_SetRRC_MessageSN_REQ

RRC LLA @ 00:13:23.360

Channel ID: Rb0
Cell ID: 0

Message Details:

CRLC_SetRRC_MessageSN_REQ:

cellId:0

routingInfo:

rB_Identity:0

count_I_LSB_UL (RRC_SequenceNumber): Omit
count_I_LSB_DL (RRC_SequenceNumber):0

#### PHY_DATA_IND

PHY MAC @ 00:13:23.380

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 199

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 03 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### MAC_DATA_IND

MAC RLC @ 00:13:23.380

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 199

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:3

#### CRLC_SetRRC_MessageSN_CNF

LLA RRC @ 00:13:23.380

Channel ID: Rb0
Cell ID: 0

Message Details:

CRLC_SetRRC_MessageSN_CNF:

cellId:0

routingInfo:

rB_Identity:0

#### CRLC_SetRRC_MessageSN_REQ

RRC LLA @ 00:13:23.380

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_REQ:

cellId:-1

routingInfo:

rB_Identity:1

count_I_LSB_UL (RRC_SequenceNumber): Omit
count_I_LSB_DL (RRC_SequenceNumber):0

#### CRLC_SetRRC_MessageSN_CNF

LLA RRC @ 00:13:23.390

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_CNF:

cellId:-1

routingInfo:

rB_Identity:1

#### CRLC_SetRRC_MessageSN_REQ

RRC LLA @ 00:13:23.390

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_REQ:

cellId:-1

routingInfo:

rB_Identity:2

count_I_LSB_UL (RRC_SequenceNumber): Omit
count_I_LSB_DL (RRC_SequenceNumber):0

#### CRLC_SetRRC_MessageSN_CNF

LLA RRC @ 00:13:23.410

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_CNF:

cellId:-1

routingInfo:

rB_Identity:2

#### CRLC_SetRRC_MessageSN_REQ

RRC LLA @ 00:13:23.410

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_REQ:

cellId:-1

routingInfo:

rB_Identity:3

count_I_LSB_UL (RRC_SequenceNumber): Omit
count_I_LSB_DL (RRC_SequenceNumber):0

#### CRLC_SetRRC_MessageSN_CNF

LLA RRC @ 00:13:23.430

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_CNF:

cellId:-1

routingInfo:

rB_Identity:3

#### CRLC_SetRRC_MessageSN_REQ

RRC LLA @ 00:13:23.430

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_REQ:

cellId:-1

routingInfo:

rB_Identity:4

count_I_LSB_UL (RRC_SequenceNumber): Omit
count_I_LSB_DL (RRC_SequenceNumber):0

#### CRLC_SetRRC_MessageSN_CNF

LLA RRC @ 00:13:23.440

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_CNF:

cellId:-1

routingInfo:

rB_Identity:4

#### CRLC_Integrity_Activate_REQ

RRC LLA @ 00:13:23.440

Cell ID: -1

Message Details:

CRLC_Integrity_Activate_REQ:

cellId:-1
cn_DomainIdentity:cs_domain

integrityActivationInfo:

integrityProtectionModeInfo:

integrityProtectionModeCommand:

startIntegrityProtection:

integrityProtInitNumber:00001111000011110000111100001111

integrityProtectionAlgorithm:uia1

#### CRLC_Integrity_Activate_REQ

RRC RLC @ 00:13:23.440

Message Details:

cellIdentity: 1

integrityActivationInfo:

integrityProtectionModeInfo:

integrityProtectionModeCommand:

startIntegrityProtection:

integrityProtInitNumber: 00001111000011110000111100001111

#### CRLC_Integrity_Activate_CNF

LLA RRC @ 00:13:23.460

Cell ID: -1

Message Details:

CRLC_Integrity_Activate_CNF:

cellId:-1

#### CRLC_Integrity_Activate_REQ

RRC LLA @ 00:13:23.460

Cell ID: -1

Message Details:

CRLC_Integrity_Activate_REQ:

cellId:-1
cn_DomainIdentity:cs_domain

integrityActivationInfo:

ul_IntegProtActivationInfo: (IntegrityProtActivationInfoList)

SS_IntegrityProtActivationTimeInfo:

rb_Identity:2
rrc_MessageSequenceNumber:0

#### CRLC_Integrity_Activate_REQ

RRC RLC @ 00:13:23.460

Message Details:

cellIdentity: 1

integrityActivationInfo:

ul_IntegrityProtActivationInfo:

rrc_MessageSequenceNumberList:

RRC_MessageSequenceNumberList.element: -2

RRC_MessageSequenceNumberList.element: -2

RRC_MessageSequenceNumberList.element: 0

RRC_MessageSequenceNumberList.element: -2

RRC_MessageSequenceNumberList.element: -2

#### CMAC Integrity Check Request

RRC MAC @ 00:13:23.470

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000001
Data:

[0]00 00 00 01
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:1 (RNC to UE)
Message Length (bits):128
Message:

[0]80 00 00 01 04 06 00 01
[8]80 01 41 E1 E1 E1 E0 18

#### CMAC Integrity Check Result

MAC RRC @ 00:13:23.470

Message Details:

Integrity Check Result:

MAC-I:11001111110011000100010011001110
Data:

[0]CF CC 44 CE

#### CRLC_Integrity_Activate_CNF

LLA RRC @ 00:13:23.470

Cell ID: -1

Message Details:

CRLC_Integrity_Activate_CNF:

cellId:-1

#### RLC_AM_DATA_REQ

RRC LLA @ 00:13:23.470

Channel ID: Rb2
Cell ID: -1

Message Details:

RLC_AM_DATA_REQ:

cellId:-1

routingInfo:

rB_Identity:2

confirmationRequest: (AmConfirmationRequest)

noConfirmationRequest:

aM_message:

dL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode:00000000000000000000000000000000
rrc_MessageSequenceNumber:0

message: (DL_DCCH_MessageType)

securityModeCommand:

r3:

securityModeCommand_r3: (SecurityModeCommand_r3_IEs)

rrc_TransactionIdentifier:0

securityCapability:

cipheringAlgorithmCap:0000000000000011
integrityProtectionAlgorithmCap:0000000000000010

cipheringModeInfo: Omit

integrityProtectionModeInfo:

integrityProtectionModeCommand:

startIntegrityProtection:

integrityProtInitNumber:00001111000011110000111100001111

integrityProtectionAlgorithm:uia1

cn_DomainIdentity:cs_domain

ue_SystemSpecificSecurityCap: (InterRAT_UE_SecurityCapList)

InterRAT_UE_SecurityCapability:

gsm:

gsmSecurityCapability:0000011

laterNonCriticalExtensions: Omit

#### RLC_AM_DATA_REQ: securityModeCommand

LLA RLC @ 00:13:23.470

Channel No: 2 Name: DCCH

Message Details:

DL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode: 11001111110011000100010011001110

rrc_MessageSequenceNumber: 1

message:

securityModeCommand:

r3:

securityModeCommand_r3:

rrc_TransactionIdentifier: 0

securityCapability:

cipheringAlgorithmCap: 0000000000000011

integrityProtectionAlgorithmCap: 0000000000000010

cipheringModeInfo: Omitted

integrityProtectionModeInfo:

integrityProtectionModeCommand:

startIntegrityProtection:

integrityProtInitNumber: 00001111000011110000111100001111

integrityProtectionAlgorithm: uia1_IntegrityProtectionAlgorithm [enum=0]

cn_DomainIdentity: cs_domain_CN_DomainIdentity [enum=0]

ue_SystemSpecificSecurityCap:

InterRAT_UE_SecurityCapList.element:

gsm:

gsmSecurityCapability: 0000011

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]E7 E6 22 67 0C 06 00 01
[8]80 01 41 E1 E1 E1 E0 18

#### MAC_DATA_REQ

RLC MAC @ 00:13:23.480

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 229

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 00 E7 E6 22 67 0C 06
[8]00 01 80 01 41 E1 E1 E1
[16]E0 18

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:0
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]E7 E6 22 67 0C 06 00 01
[8]80 01 41 E1 E1 E1 E0 18

#### MAC_DATA_REQ

RLC MAC @ 00:13:23.480

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 229

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 0D 01 FE 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:1
Polling bit:1 (request a status report)
Length indicator 0 (octets):0 (the previous RLC PDU was exactly filled by the last segment of an RLC SDU)
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (0 octets):

Padding associated with length indicator 1 (14 octets):

[0]00 00 00 00 00 00 00 00
[8]00 00 00 00 00 00

#### PHY_DATA_REQ

MAC PHY @ 00:13:23.480

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 229

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 00 0E 7E 62 26 70 C0
[8]60 00 18 00 14 1E 1E 1E
[16]1E 01 80 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 00 E7 E6 22 67 0C 06
[8]00 01 80 01 41 E1 E1 E1
[16]E0 18

#### PHY_DATA_REQ

MAC PHY @ 00:13:23.490

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 230

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 00 D0 1F E0 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 0D 01 FE 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:13:23.530

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 214

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 01 51 E6 C0 05 82 AA
[8]2A A2 3B B3 10 82 08 80
[16]19 91 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 15 1E 6C 00 58 2A A2
[8]AA 23 BB 31 08 20 88 01
[16]99 10

#### MAC_DATA_IND

MAC RLC @ 00:13:23.530

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 214

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 15 1E 6C 00 58 2A A2
[8]AA 23 BB 31 08 20 88 01
[16]99 10

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:2
Polling bit:1 (request a status report)
Length indicator 0 (octets):15
Segment associated with length indicator 0 (15 octets):

[0]6C 00 58 2A A2 AA 23 BB
[8]31 08 20 88 01 99 10

#### MAC_DATA_REQ

RLC MAC @ 00:13:23.540

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 235

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:3

#### PHY_DATA_REQ

MAC PHY @ 00:13:23.540

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 235

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 03 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### MAC_DATA_REQ

RLC MAC @ 00:13:23.680

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 249

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 0D 01 FE 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:1
Polling bit:1 (request a status report)
Length indicator 0 (octets):0 (the previous RLC PDU was exactly filled by the last segment of an RLC SDU)
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (0 octets):

Padding associated with length indicator 1 (14 octets):

[0]00 00 00 00 00 00 00 00
[8]00 00 00 00 00 00

#### PHY_DATA_REQ

MAC PHY @ 00:13:23.680

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 249

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 00 D0 1F E0 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 0D 01 FE 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:13:23.720

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 233

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]10 20 02 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]02 00 20 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### MAC_DATA_IND

MAC RLC @ 00:13:23.720

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 233

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 20 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:2

#### PHY_DATA_IND

PHY MAC @ 00:13:23.730

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 234

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 01 D1 3F EC 59 1B E7
[8]10 D2 10 00 00 05 55 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 1D 13 FE C5 91 BE 71
[8]0D 21 00 00 00 55 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:13:23.730

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 234

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 1D 13 FE C5 91 BE 71
[8]0D 21 00 00 00 55 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:3
Polling bit:1 (request a status report)
Length indicator 0 (octets):9
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (9 octets):

[0]C5 91 BE 71 0D 21 00 00
[8]00
Padding associated with length indicator 1 (5 octets):

[0]55 55 55 55 55

#### MAC_DATA_REQ

RLC MAC @ 00:13:23.740

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 255

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 40 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:4

#### PHY_DATA_REQ

MAC PHY @ 00:13:23.740

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 255

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]10 20 04 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]02 00 40 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### CMAC Integrity Check Request

RRC MAC @ 00:13:23.770

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000001
Data:

[0]00 00 00 01
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:0 (UE to RNC)
Message Length (bits):72
Message:

[0]80 00 00 01 05 21 00 00
[8]00

#### RLC_AM_DATA_IND: securityModeComplete

RLC LLA @ 00:13:23.770

Channel No: 2 Name: DCCH

Message Details:

UL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode: 10001011001000110111110011100010

rrc_MessageSequenceNumber: 1

message:

securityModeComplete:

rrc_TransactionIdentifier: 0

ul_IntegProtActivationInfo:

rrc_MessageSequenceNumberList:

RRC_MessageSequenceNumberList.element: 0

RRC_MessageSequenceNumberList.element: 0

RRC_MessageSequenceNumberList.element: 0

RRC_MessageSequenceNumberList.element: 0

RRC_MessageSequenceNumberList.element: 0

rb_UL_CiphActivationTimeInfo: Omitted

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]C5 91 BE 71 0D 21 00 00
[8]00

#### CMAC Integrity Check Result

MAC RRC @ 00:13:23.770

Message Details:

Integrity Check Result:

MAC-I:10001011001000110111110011100010
Data:

[0]8B 23 7C E2

#### RLC_AM_DATA_IND

LLA RRC @ 00:13:23.770

Channel ID: Rb2
Cell ID: -1

Message Details:

RLC_AM_DATA_IND:

cellId:-1

routingInfo:

rB_Identity:2

integrityResult:

integrityUsed (IntegrityStatus):i_pass

aM_message:

uL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode:10001011001000110111110011100010
rrc_MessageSequenceNumber:1

message: (UL_DCCH_MessageType)

securityModeComplete:

rrc_TransactionIdentifier:0

ul_IntegProtActivationInfo: (IntegrityProtActivationInfo)

rrc_MessageSequenceNumberList:

RRC_MessageSequenceNumber:0
RRC_MessageSequenceNumber:0
RRC_MessageSequenceNumber:0
RRC_MessageSequenceNumber:0
RRC_MessageSequenceNumber:0

rb_UL_CiphActivationTimeInfo: (RB_ActivationTimeInfoList) Omit

laterNonCriticalExtensions: Omit

#### CRLC_Integrity_Activate_REQ

RRC LLA @ 00:13:23.770

Cell ID: -1

Message Details:

CRLC_Integrity_Activate_REQ:

cellId:-1
cn_DomainIdentity:cs_domain

integrityActivationInfo:

ul_IntegProtActivationInfo: (IntegrityProtActivationInfoList)

SS_IntegrityProtActivationTimeInfo:

rb_Identity:0
rrc_MessageSequenceNumber:0

SS_IntegrityProtActivationTimeInfo:

rb_Identity:1
rrc_MessageSequenceNumber:0

SS_IntegrityProtActivationTimeInfo:

rb_Identity:3
rrc_MessageSequenceNumber:0

SS_IntegrityProtActivationTimeInfo:

rb_Identity:4
rrc_MessageSequenceNumber:0

#### CRLC_Integrity_Activate_REQ

RRC RLC @ 00:13:23.770

Message Details:

cellIdentity: 1

integrityActivationInfo:

ul_IntegrityProtActivationInfo:

rrc_MessageSequenceNumberList:

RRC_MessageSequenceNumberList.element: 0

RRC_MessageSequenceNumberList.element: 0

RRC_MessageSequenceNumberList.element: -2

RRC_MessageSequenceNumberList.element: 0

RRC_MessageSequenceNumberList.element: 0

#### CMAC Integrity Check Request

RRC MAC @ 00:13:23.790

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000001
Data:

[0]00 00 00 01
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:1 (RNC to UE)
Message Length (bits):192
Message:

[0]80 00 00 01 81 40 01 E0
[8]A0 40 1E 22 00 00 22 E0
[16]BE 82 24 46 68 94 34 40

#### CMAC Integrity Check Result

MAC RRC @ 00:13:23.790

Message Details:

Integrity Check Result:

MAC-I:00010011010010000100010001011010
Data:

[0]13 48 44 5A

#### CRLC_Integrity_Activate_CNF

LLA RRC @ 00:13:23.790

Cell ID: -1

Message Details:

CRLC_Integrity_Activate_CNF:

cellId:-1

#### RRC_DATA_REQ: mm:locationUpdatingAccept

NAS RRC @ 00:13:23.790

Cell ID: -1

Message Details:

LOCATIONUPDATINGACCEPT:

skipIndicator: 0000

mMProtocolDiscriminator: 0101

msgType: 00000010

locAreaId:

plmn: 00F110

lac: 0001

mobileId:

iei: 00010111

iel: 05

iDigit1: 1111

oddEvenInd: 0

typeOfId: 100

otherDigits: 11223344

followOnProceed: 10100001

cTSPerm: 10100010

equivalentPLMN: Omitted

#### RLC_AM_DATA_REQ:downlinkDirectTransfer

RRC RLC @ 00:13:23.790

Channel No: 3 Name: DCCH

Message Details:

Opt1: 0

Opt2: 0

DL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode: 00010011010010000100010001011010

rrc_MessageSequenceNumber: 1

message:

downlinkDirectTransfer:

r3:

downlinkDirectTransfer_r3:

rrc_TransactionIdentifier: 0

cn_DomainIdentity: cs_domain_CN_DomainIdentity [enum=0]

nas_Message: 050200F11000011705F411223344A1A2

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]89 A4 22 2D 09 40 01 E0
[8]A0 40 1E 22 00 00 22 E0
[16]BE 82 24 46 68 94 34 40

#### MAC_DATA_REQ

RLC MAC @ 00:13:23.790

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 4

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 18 89 A4 22 2D 09 40
[8]01 E0 A0 40 1E 22 00 00
[16]22 E0

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:3
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]89 A4 22 2D 09 40 01 E0
[8]A0 40 1E 22 00 00 22 E0

#### MAC_DATA_REQ

RLC MAC @ 00:13:23.790

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 4

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 25 11 FE BE 82 24 46
[8]68 94 34 40 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:4
Polling bit:1 (request a status report)
Length indicator 0 (octets):8
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (8 octets):

[0]BE 82 24 46 68 94 34 40
Padding associated with length indicator 1 (6 octets):

[0]00 00 00 00 00 00

#### PHY_DATA_REQ

MAC PHY @ 00:13:23.790

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 4

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 01 88 9A 42 22 D0 94
[8]00 1E 0A 04 01 E2 20 00
[16]02 2E 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 18 89 A4 22 2D 09 40
[8]01 E0 A0 40 1E 22 00 00
[16]22 E0

#### PHY_DATA_REQ

MAC PHY @ 00:13:23.800

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 5

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 02 51 1F EB E8 22 44
[8]66 89 43 44 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 25 11 FE BE 82 24 46
[8]68 94 34 40 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:13:23.930

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 254

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]10 20 02 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]02 00 20 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### MAC_DATA_IND

MAC RLC @ 00:13:23.930

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 254

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 20 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:2

#### PHY_DATA_IND

PHY MAC @ 00:13:23.940

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 255

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 01 D1 3F EC 59 1B E7
[8]10 D2 10 00 00 05 55 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 1D 13 FE C5 91 BE 71
[8]0D 21 00 00 00 55 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:13:23.940

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 255

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 1D 13 FE C5 91 BE 71
[8]0D 21 00 00 00 55 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:3
Polling bit:1 (request a status report)
Length indicator 0 (octets):9
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (9 octets):

[0]C5 91 BE 71 0D 21 00 00
[8]00
Padding associated with length indicator 1 (5 octets):

[0]55 55 55 55 55

#### MAC_DATA_REQ

RLC MAC @ 00:13:23.950

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 20

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 40 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:4

#### PHY_DATA_REQ

MAC PHY @ 00:13:23.950

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 20

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]10 20 04 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]02 00 40 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### MAC_DATA_REQ

RLC MAC @ 00:13:23.990

Category: Configuration
BTS unit: 1:?
Channel No: 3 Name: DCCH
CFN: 24

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 25 11 FE BE 82 24 46
[8]68 94 34 40 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:4
Polling bit:1 (request a status report)
Length indicator 0 (octets):8
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (8 octets):

[0]BE 82 24 46 68 94 34 40
Padding associated with length indicator 1 (6 octets):

[0]00 00 00 00 00 00

#### PHY_DATA_REQ

MAC PHY @ 00:13:23.990

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 24

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 02 51 1F EB E8 22 44
[8]66 89 43 44 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 25 11 FE BE 82 24 46
[8]68 94 34 40 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:13:24.030

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 8

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 05 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 50 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### MAC_DATA_IND

MAC RLC @ 00:13:24.030

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 8

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 50 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:5

#### PHY_DATA_IND

PHY MAC @ 00:13:24.040

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 9

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 01 D1 5F EA 4D 81 B8
[8]D8 EC 00 08 2C D8 05 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 1D 15 FE A4 D8 1B 8D
[8]8E C0 00 82 CD 80 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:13:24.040

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 9

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 1D 15 FE A4 D8 1B 8D
[8]8E C0 00 82 CD 80 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:3
Polling bit:1 (request a status report)
Length indicator 0 (octets):10
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (10 octets):

[0]A4 D8 1B 8D 8E C0 00 82
[8]CD 80
Padding associated with length indicator 1 (4 octets):

[0]55 55 55 55

#### RLC_AM_DATA_IND: uplinkDirectTransfer

RLC RRC @ 00:13:24.050

Channel No: 3 Name: DCCH

Message Details:

UL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode: 01001001101100000011011100011011

rrc_MessageSequenceNumber: 1

message:

uplinkDirectTransfer:

cn_DomainIdentity: cs_domain_CN_DomainIdentity [enum=0]

nas_Message: 059B

measuredResultsOnRACH: Omitted

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]A4 D8 1B 8D 8E C0 00 82
[8]CD 80

#### RRC_DATA_IND: mm:tmsiReallocationComplete

RRC NAS @ 00:13:24.050

Cell ID: -1

Message Details:

TMSIREALLOCATIONCOMPLETE:

skipIndicator: 0000

mMProtocolDiscriminator: 0101

msgType: 10011011

#### MAC_DATA_REQ

RLC MAC @ 00:13:24.050

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 30

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 40 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:4

#### PHY_DATA_REQ

MAC PHY @ 00:13:24.050

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 30

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 04 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 40 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### CMAC Integrity Check Request

RRC MAC @ 00:13:24.080

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000001
Data:

[0]00 00 00 01
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:0 (UE to RNC)
Message Length (bits):80
Message:

[0]80 00 00 01 86 C0 00 82
[8]CD 80

#### CMAC Integrity Check Result

MAC RRC @ 00:13:24.080

Message Details:

Integrity Check Result:

MAC-I:01001001101100000011011100011011
Data:

[0]49 B0 37 1B

#### PHY_DATA_IND

PHY MAC @ 00:13:24.240

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 29

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 05 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 50 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### MAC_DATA_IND

MAC RLC @ 00:13:24.240

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 29

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 50 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:5

#### PHY_DATA_IND

PHY MAC @ 00:13:24.250

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 30

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 01 D1 5F EA 4D 81 B8
[8]D8 EC 00 08 2C D8 05 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 1D 15 FE A4 D8 1B 8D
[8]8E C0 00 82 CD 80 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:13:24.250

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 30

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 1D 15 FE A4 D8 1B 8D
[8]8E C0 00 82 CD 80 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:3
Polling bit:1 (request a status report)
Length indicator 0 (octets):10
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (10 octets):

[0]A4 D8 1B 8D 8E C0 00 82
[8]CD 80
Padding associated with length indicator 1 (4 octets):

[0]55 55 55 55

#### MAC_DATA_REQ

RLC MAC @ 00:13:24.260

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 51

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 40 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:4

#### PHY_DATA_REQ

MAC PHY @ 00:13:24.260

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 51

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 04 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 40 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### CMAC Integrity Check Request

RRC MAC @ 00:13:25.100

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000001
Data:

[0]00 00 00 01
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:1 (RNC to UE)
Message Length (bits):56
Message:

[0]80 00 00 00 83 C8 00

#### CMAC Integrity Check Result

MAC RRC @ 00:13:25.100

Message Details:

Integrity Check Result:

MAC-I:11101100100111000001011111010011
Data:

[0]EC 9C 17 D3

#### RLC_UM_DATA_REQ

RRC LLA @ 00:13:25.100

Channel ID: Rb1
Cell ID: -1

Message Details:

RLC_UM_DATA_REQ:

cellId:-1

routingInfo:

rB_Identity:1

uM_message:

dL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode:00000000000000000000000000000000
rrc_MessageSequenceNumber:0

message: (DL_DCCH_MessageType)

rrcConnectionRelease:

r3:

rrcConnectionRelease_r3: (RRCConnectionRelease_r3_IEs)

rrc_TransactionIdentifier:0
n_308:1
releaseCause:normalEvent

rplmn_information: Omit

laterNonCriticalExtensions: Omit

specialLI:false

#### RLC_UM_DATA_REQ: rrcConnectionRelease

LLA RLC @ 00:13:25.100

Channel No: 1 Name: DCCH

Message Details:

DL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode: 11101100100111000001011111010011

rrc_MessageSequenceNumber: 1

message:

rrcConnectionRelease:

r3:

rrcConnectionRelease_r3:

rrc_TransactionIdentifier: 0

n_308: 1

releaseCause: normalEvent_ReleaseCause [enum=0]

rplmn_information: Omitted

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]F6 4E 0B E9 8B C8 00

#### MAC_DATA_REQ

RLC MAC @ 00:13:25.100

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 135

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]01 0F FE F6 4E 0B E9 8B
[8]C8 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

Sequence number:0
Length indicator 0 (octets):7
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (7 octets):

[0]F6 4E 0B E9 8B C8 00
Padding associated with length indicator 1 (8 octets):

[0]00 00 00 00 00 00 00 00

#### PHY_DATA_REQ

MAC PHY @ 00:13:25.100

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 135

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]00 10 FF EF 64 E0 BE 98
[8]BC 80 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:0
MAC SDU (144 bits):

[0]01 0F FE F6 4E 0B E9 8B
[8]C8 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:13:25.340

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 139

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]00 10 DF EF BF 16 16 70
[8]C4 05 55 55 55 55 55 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:0
MAC SDU (144 bits):

[0]01 0D FE FB F1 61 67 0C
[8]40 55 55 55 55 55 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:13:25.340

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 139

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]01 0D FE FB F1 61 67 0C
[8]40 55 55 55 55 55 55 55
[16]55 55

RLC PDU (decoded):

Sequence number:0
Length indicator 0 (octets):6
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (6 octets):

[0]FB F1 61 67 0C 40
Padding associated with length indicator 1 (9 octets):

[0]55 55 55 55 55 55 55 55
[8]55

#### CMAC Integrity Check Request

RRC MAC @ 00:13:25.360

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000001
Data:

[0]00 00 00 01
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:0 (UE to RNC)
Message Length (bits):48
Message:

[0]80 00 00 00 84 40

#### RLC_UM_DATA_IND: rrcConnectionReleaseComplete

RLC LLA @ 00:13:25.360

Channel No: 1 Name: DCCH

Message Details:

UL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode: 11110111111000101100001011001110

rrc_MessageSequenceNumber: 1

message:

rrcConnectionReleaseComplete:

rrc_TransactionIdentifier: 0

errorIndication: Omitted

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]FB F1 61 67 0C 40

#### CMAC Integrity Check Result

MAC RRC @ 00:13:25.360

Message Details:

Integrity Check Result:

MAC-I:11110111111000101100001011001110
Data:

[0]F7 E2 C2 CE

#### RLC_UM_DATA_IND

LLA RRC @ 00:13:25.360

Channel ID: Rb1
Cell ID: -1

Message Details:

RLC_UM_DATA_IND:

cellId:-1

routingInfo:

rB_Identity:1

integrityResult:

integrityUsed (IntegrityStatus):i_pass

uM_message:

uL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode:11110111111000101100001011001110
rrc_MessageSequenceNumber:1

message: (UL_DCCH_MessageType)

rrcConnectionReleaseComplete:

rrc_TransactionIdentifier:0

errorIndication: (FailureCauseWithProtErr) Omit

laterNonCriticalExtensions: Omit

#### PHY_DATA_IND

PHY MAC @ 00:13:25.500

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 155

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]00 30 DF ED CD 18 3E 01
[8]44 05 55 55 55 55 55 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:0
MAC SDU (144 bits):

[0]03 0D FE DC D1 83 E0 14
[8]40 55 55 55 55 55 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:13:25.500

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 155

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]03 0D FE DC D1 83 E0 14
[8]40 55 55 55 55 55 55 55
[16]55 55

RLC PDU (decoded):

Sequence number:1
Length indicator 0 (octets):6
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (6 octets):

[0]DC D1 83 E0 14 40
Padding associated with length indicator 1 (9 octets):

[0]55 55 55 55 55 55 55 55
[8]55

#### CMAC Integrity Check Request

RRC MAC @ 00:13:25.540

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000010
Data:

[0]00 00 00 02
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:0 (UE to RNC)
Message Length (bits):48
Message:

[0]80 00 00 00 84 40

#### RLC_UM_DATA_IND: rrcConnectionReleaseComplete

RLC LLA @ 00:13:25.540

Channel No: 1 Name: DCCH

Message Details:

UL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode: 10111001101000110000011111000000

rrc_MessageSequenceNumber: 2

message:

rrcConnectionReleaseComplete:

rrc_TransactionIdentifier: 0

errorIndication: Omitted

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]DC D1 83 E0 14 40

#### CMAC Integrity Check Result

MAC RRC @ 00:13:25.540

Message Details:

Integrity Check Result:

MAC-I:10111001101000110000011111000000
Data:

[0]B9 A3 07 C0

#### RLC_UM_DATA_IND

LLA RRC @ 00:13:25.540

Channel ID: Rb1
Cell ID: -1

Message Details:

RLC_UM_DATA_IND:

cellId:-1

routingInfo:

rB_Identity:1

integrityResult:

integrityUsed (IntegrityStatus):i_pass

uM_message:

uL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode:10111001101000110000011111000000
rrc_MessageSequenceNumber:2

message: (UL_DCCH_MessageType)

rrcConnectionReleaseComplete:

rrc_TransactionIdentifier:0

errorIndication: (FailureCauseWithProtErr) Omit

laterNonCriticalExtensions: Omit

#### CRLC_Config_REQ

RRC LLA @ 00:13:25.540

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:1

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC UM Channel Release REQ

LLA RLC @ 00:13:25.540

BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 179

Message Details:

#### CRLC UM Channel Release CNF

RLC LLA @ 00:13:25.540

BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 179

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:13:25.550

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:1

#### CRLC_Config_REQ

RRC LLA @ 00:13:25.550

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:2

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC AM Channel Release REQ

LLA RLC @ 00:13:25.550

BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 180

Message Details:

#### CRLC AM Channel Release CNF

RLC LLA @ 00:13:25.550

BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 180

Message Details:

#### CRLC AM Channel Release REQ

LLA RLC @ 00:13:25.560

BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 181

Message Details:

#### CRLC AM Channel Release CNF

RLC LLA @ 00:13:25.560

BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 181

Message Details:

#### CPHY_OUTSYNC_IND

PHY RRC @ 00:13:25.560

BTS unit: 1:1
Channel No: 0 Name: U_DPCH
CFN: 181

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:13:25.570

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:2

#### CRLC_Config_REQ

RRC LLA @ 00:13:25.570

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:3

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC_Config_CNF

LLA RRC @ 00:13:25.580

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:3

#### CRLC_Config_REQ

RRC LLA @ 00:13:25.580

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:4

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC AM Channel Release REQ

LLA RLC @ 00:13:25.580

BTS unit: 1:1
Channel No: 4 Name: DCCH
CFN: 183

Message Details:

#### CRLC AM Channel Release CNF

RLC LLA @ 00:13:25.580

BTS unit: 1:1
Channel No: 4 Name: DCCH
CFN: 183

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:13:25.600

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:4

#### CRLC_Config_REQ

RRC LLA @ 00:13:25.600

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:1

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode)

dl_UM_RLC_Mode:

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):136

dl_RLCModeInfo: (UL_RLC_Mode)

ul_UM_RLC_Mode:

transmissionRLC_Discard:

timerBasedNoExplicit (NoExplicitDiscard):dt100

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity):1
dLlogicalChannelIdentity (LogicalChannelIdentity):1
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC UM Channel Establish REQ

LLA RLC @ 00:13:25.600

BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 185

Message Details:

Configuration Parameters:

PU Size In Bits:136

#### CRLC UM Channel Establish CNF

RLC LLA @ 00:13:25.600

BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 185

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:13:25.610

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:1

#### CRLC_Config_REQ

RRC LLA @ 00:13:25.610

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:2

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode)

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):128

dl_RLCModeInfo: (UL_RLC_Mode)

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity):2
dLlogicalChannelIdentity (LogicalChannelIdentity):2
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC AM Channel Establish REQ

LLA RLC @ 00:13:25.610

BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 186

Message Details:

Configuration Parameters:

PU Size In Bits:128

Timer Parameters:

Poll (ms):200
Poll Prohibit (ms):0
EPC (ms):0
Discard (ms):0
Poll Periodic (ms):0
Status Prohibit (ms):0
Status Periodic (ms):0
Reset (ms):500
MRW (ms):0

Protocol Parameters:

Max Dat:15
Poll PU:0
Poll SDU:1
Poll Window:99
Max Reset:1
Tx Window Size:32
Rx Window Size:32
Max MRW:0
SDU Discard Mode:No discard

Polling Triggers:

Last PU In Buffer:On
Last PU In Retransmission Buffer:On
Poll Timer:On
Every Poll-PU PU:Off
Every Poll-SDU SDU:On
Poll-Window Percent Of Transmission Buffer:On
Timer Based:Off

Status Triggers:

Missing PU:On
Timer Based:Off
EPC Mechanism:Off

#### CRLC AM Channel Establish CNF

RLC LLA @ 00:13:25.610

BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 186

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:13:25.630

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:2

#### CRLC_Config_REQ

RRC LLA @ 00:13:25.630

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:3

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode)

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):128

dl_RLCModeInfo: (UL_RLC_Mode)

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity):3
dLlogicalChannelIdentity (LogicalChannelIdentity):3
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC AM Channel Establish REQ

LLA RLC @ 00:13:25.630

BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 188

Message Details:

Configuration Parameters:

PU Size In Bits:128

Timer Parameters:

Poll (ms):200
Poll Prohibit (ms):0
EPC (ms):0
Discard (ms):0
Poll Periodic (ms):0
Status Prohibit (ms):0
Status Periodic (ms):0
Reset (ms):500
MRW (ms):0

Protocol Parameters:

Max Dat:15
Poll PU:0
Poll SDU:1
Poll Window:99
Max Reset:1
Tx Window Size:32
Rx Window Size:32
Max MRW:0
SDU Discard Mode:No discard

Polling Triggers:

Last PU In Buffer:On
Last PU In Retransmission Buffer:On
Poll Timer:On
Every Poll-PU PU:Off
Every Poll-SDU SDU:On
Poll-Window Percent Of Transmission Buffer:On
Timer Based:Off

Status Triggers:

Missing PU:On
Timer Based:Off
EPC Mechanism:Off

#### CRLC AM Channel Establish CNF

RLC LLA @ 00:13:25.630

BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 188

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:13:25.640

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:3

#### CRLC_Config_REQ

RRC LLA @ 00:13:25.640

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:4

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode)

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):128

dl_RLCModeInfo: (UL_RLC_Mode)

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity):4
dLlogicalChannelIdentity (LogicalChannelIdentity):4
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC AM Channel Establish REQ

LLA RLC @ 00:13:25.640

BTS unit: 1:1
Channel No: 4 Name: DCCH
CFN: 189

Message Details:

Configuration Parameters:

PU Size In Bits:128

Timer Parameters:

Poll (ms):200
Poll Prohibit (ms):0
EPC (ms):0
Discard (ms):0
Poll Periodic (ms):0
Status Prohibit (ms):0
Status Periodic (ms):0
Reset (ms):500
MRW (ms):0

Protocol Parameters:

Max Dat:15
Poll PU:0
Poll SDU:1
Poll Window:99
Max Reset:1
Tx Window Size:32
Rx Window Size:32
Max MRW:0
SDU Discard Mode:No discard

Polling Triggers:

Last PU In Buffer:On
Last PU In Retransmission Buffer:On
Poll Timer:On
Every Poll-PU PU:Off
Every Poll-SDU SDU:On
Poll-Window Percent Of Transmission Buffer:On
Timer Based:Off

Status Triggers:

Missing PU:On
Timer Based:Off
EPC Mechanism:Off

#### CRLC AM Channel Establish CNF

RLC LLA @ 00:13:25.640

BTS unit: 1:1
Channel No: 4 Name: DCCH
CFN: 189

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:13:25.660

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:4

#### MMI_CmdReq

RRC LLA @ 00:13:30.680

Message Details:

MMI_CmdReq:

cmd (IA5String):Please switch off the UE

#### MMI_CmdCnf

LLA RRC @ 00:13:36.330

Message Details:

MMI_CmdCnf:

result:true
resultString (IA5String): Omit

#### PHY_DATA_IND

PHY MAC @ 00:13:39.950

BTS unit: 1:1
Channel No: 0 Name: U_RACH
CFN: 64

Message Details:

TFI:0
TB set size:168
TB size:168
TB set (raw):

[0]08 44 48 8C D1 00 04 02
[8]00 02 D0 00 00 00 00 00
[16]00 00 00 00 00 00

TB set (decoded):

TB 0:

TCTF:0
MAC SDU (166 bits):

[0]21 11 22 33 44 00 10 08
[8]00 0B 40 00 00 00 00 00
[16]00 00 00 00 00

#### MAC_DATA_IND

MAC RLC @ 00:13:39.950

Category: Configuration
BTS unit: 1:1
Channel No: 0 Name: CCCH
CFN: 64

Message Details:

RLC PDU size (bits):166
RLC PDU (raw):

[0]21 11 22 33 44 00 10 08
[8]00 0B 40 00 00 00 00 00
[16]00 00 00 00 00

#### RLC_TR_DATA_IND: rrcConnectionRequest

RLC LLA @ 00:13:39.970

Channel No: 0 Name: CCCH

Message Details:

UL_CCCH_Message:

integrityCheckInfo: Omitted

message:

rrcConnectionRequest:

initialUE_Identity:

tmsi_and_LAI:

tmsi: 00010001001000100011001101000100

lai:

plmn_Identity:

mcc:

MCC.element: 0

MCC.element: 0

MCC.element: 1

mnc:

MNC.element: 0

MNC.element: 1

lac: 0000000000000001

establishmentCause: detach_EstablishmentCause [enum=13]

protocolErrorIndicator: noError_ProtocolErrorIndicator [enum=0]

measuredResultsOnRACH: Omitted

v3d0NonCriticalExtensions: Omitted

Layer 3 SDU:

[0]21 11 22 33 44 00 10 08
[8]00 0B 40 00 00 00 00 00
[16]00 00 00 00 00

#### RLC_TR_DATA_IND

LLA RRC @ 00:13:39.970

Channel ID: Rb0
Cell ID: 0

Message Details:

RLC_TR_DATA_IND:

cellId:0

routingInfo:

rB_Identity:0

tM_message:

uL_CCCH_Message:

integrityCheckInfo: Omit

message: (UL_CCCH_MessageType)

rrcConnectionRequest:

initialUE_Identity:

tmsi_and_LAI: (TMSI_and_LAI_GSM_MAP)

tmsi (TMSI_GSM_MAP):00010001001000100011001101000100

lai:

plmn_Identity:

mcc:

Digit:0
Digit:0
Digit:1

mnc:

Digit:0
Digit:1

lac:0000000000000001

establishmentCause:detach
protocolErrorIndicator:noError

measuredResultsOnRACH: Omit

v3d0NonCriticalExtensions: Omit

#### RLC_UM_DATA_REQ

RRC LLA @ 00:13:39.970

Channel ID: Rb0
Cell ID: 0

Message Details:

RLC_UM_DATA_REQ:

cellId:0

routingInfo:

rB_Identity:0

uM_message:

dL_CCCH_Message:

integrityCheckInfo: Omit

message: (DL_CCCH_MessageType)

rrcConnectionSetup:

r3:

rrcConnectionSetup_r3: (RRCConnectionSetup_r3_IEs)

initialUE_Identity:

tmsi_and_LAI: (TMSI_and_LAI_GSM_MAP)

tmsi (TMSI_GSM_MAP):00010001001000100011001101000100

lai:

plmn_Identity:

mcc:

Digit:0
Digit:0
Digit:1

mnc:

Digit:0
Digit:1

lac:0000000000000001

rrc_TransactionIdentifier:0
activationTime: Omit

new_U_RNTI: (U_RNTI)

srnc_Identity:000000000001
s_RNTI:00000000000000000001

new_c_RNTI (C_RNTI): Omit
rrc_StateIndicator:cell_DCH
utran_DRX_CycleLengthCoeff (UTRAN_DRX_CycleLengthCoefficient):9

capabilityUpdateRequirement:

ue_RadioCapabilityFDDUpdateRequirement:true
ue_RadioCapabilityTDDUpdateRequirement:false

systemSpecificCapUpdateReqList:

SystemSpecificCapUpdateReq:gsm

srb_InformationSetupList: (SRB_InformationSetupList2)

SRB_InformationSetup:

rb_Identity: Omit

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_UM_RLC_Mode:

transmissionRLC_Discard: Omit

dl_RLC_Mode:

dl_UM_RLC_Mode:

rb_MappingInfo:

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

dch (TransportChannelIdentity):5

logicalChannelIdentity:1

rlc_SizeList:

configured:

mac_LogicalChannelPriority:1

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

dch (TransportChannelIdentity):10

logicalChannelIdentity:1

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

rach:

logicalChannelIdentity:1

rlc_SizeList:

explicitList: (RLC_SizeExplicitList)

RLC_SizeInfo:

rlc_SizeIndex:1

mac_LogicalChannelPriority:1

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

fach:

logicalChannelIdentity:1

SRB_InformationSetup:

rb_Identity: Omit

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

rb_MappingInfo:

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

dch (TransportChannelIdentity):5

logicalChannelIdentity:2

rlc_SizeList:

configured:

mac_LogicalChannelPriority:2

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

dch (TransportChannelIdentity):10

logicalChannelIdentity:2

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

rach:

logicalChannelIdentity:2

rlc_SizeList:

explicitList: (RLC_SizeExplicitList)

RLC_SizeInfo:

rlc_SizeIndex:1

mac_LogicalChannelPriority:2

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

fach:

logicalChannelIdentity:2

SRB_InformationSetup:

rb_Identity: Omit

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

rb_MappingInfo:

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

dch (TransportChannelIdentity):5

logicalChannelIdentity:3

rlc_SizeList:

configured:

mac_LogicalChannelPriority:3

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

dch (TransportChannelIdentity):10

logicalChannelIdentity:3

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

rach:

logicalChannelIdentity:3

rlc_SizeList:

explicitList: (RLC_SizeExplicitList)

RLC_SizeInfo:

rlc_SizeIndex:1

mac_LogicalChannelPriority:3

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

fach:

logicalChannelIdentity:3

SRB_InformationSetup:

rb_Identity: Omit

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

rb_MappingInfo:

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

dch (TransportChannelIdentity):5

logicalChannelIdentity:4

rlc_SizeList:

configured:

mac_LogicalChannelPriority:4

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

dch (TransportChannelIdentity):10

logicalChannelIdentity:4

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

rach:

logicalChannelIdentity:4

rlc_SizeList:

explicitList: (RLC_SizeExplicitList)

RLC_SizeInfo:

rlc_SizeIndex:1

mac_LogicalChannelPriority:4

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

fach:

logicalChannelIdentity:4

ul_CommonTransChInfo:

tfc_Subset: Omit

prach_TFCS: (TFCS) Omit

modeSpecificInfo:

fdd:

ul_TFCS: (TFCS)

normalTFCI_Signalling: (ExplicitTFCS_Configuration)

complete: (TFCS_ReconfAdd)

ctfcSize:

ctfc2Bit:

:

ctfc2:0

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc2:1

powerOffsetInformation:

gainFactorInformation:

signalledGainFactors:

modeSpecificInfo:

fdd:

gainFactorBetaC (GainFactor):11

gainFactorBetaD (GainFactor):15
referenceTFC_ID:0

powerOffsetPp_m: Omit

ul_AddReconfTransChInfoList:

UL_AddReconfTransChInformation:

ul_TransportChannelType (UL_TrCH_Type):dch
transportChannelIdentity:5

transportFormatSet:

dedicatedTransChTFS:

tti:

tti10: (DedicatedDynamicTF_InfoList)

DedicatedDynamicTF_Info:

rlc_Size:

bitMode: (BitModeRLC_SizeInfo)

sizeType2:

part1:2
part2: Omit

numberOfTbSizeList:

NumberOfTransportBlocks:

zero:

NumberOfTransportBlocks:

one:

logicalChannelList:

allSizes:

semistaticTF_Information:

channelCodingType:

convolutional (CodingRate):third

rateMatchingAttribute:192
crc_Size:crc16

dl_CommonTransChInfo:

sccpch_TFCS: (TFCS) Omit

modeSpecificInfo:

fdd:

dl_Parameters:

sameAsUL:

dl_AddReconfTransChInfoList:

DL_AddReconfTransChInformation:

dl_TransportChannelType (DL_TrCH_Type):dch
dl_transportChannelIdentity (TransportChannelIdentity):10

tfs_SignallingMode:

sameAsULTrCH: (UL_TransportChannelIdentity)

ul_TransportChannelType (UL_TrCH_Type):dch
ul_TransportChannelIdentity (TransportChannelIdentity):5

dch_QualityTarget: (QualityTarget)

bler_QualityValue:-20

dummy: (TM_SignallingInfo) Omit

frequencyInfo: Omit

maxAllowedUL_TX_Power: Omit

ul_ChannelRequirement:

ul_DPCH_Info:

ul_DPCH_PowerControlInfo:

fdd:

dpcch_PowerOffset:-40
pc_Preamble:1
sRB_delay:7

powerControlAlgorithm:

algorithm1 (TPC_StepSizeFDD):0

modeSpecificInfo:

fdd:

scramblingCodeType:longSC
scramblingCode (UL_ScramblingCode):0
numberOfDPDCH: Omit
spreadingFactor:sf64
tfci_Existence:true
numberOfFBI_Bits: Omit
puncturingLimit:pl1

dl_CommonInformation:

dl_DPCH_InfoCommon:

cfnHandling:

initialise:

cfntargetsfnframeoffset: Omit

modeSpecificInfo:

fdd:

dl_DPCH_PowerControlInfo:

modeSpecificInfo:

fdd:

dpc_Mode:singleTPC

powerOffsetPilot_pdpdch:0

dl_rate_matching_restriction: Omit

spreadingFactorAndPilot: (SF512_AndPilot)

sfd128 (PilotBits128):pb4

positionFixedOrFlexible:fixed
tfci_Existence:false

modeSpecificInfo:

fdd:

defaultDPCH_OffsetValue (DefaultDPCH_OffsetValueFDD):0

dpch_CompressedModeInfo: Omit

tx_DiversityMode:noDiversity

ssdt_Information: Omit

dl_InformationPerRL_List:

DL_InformationPerRL:

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode:100

pdsch_SHO_DCH_Info: Omit

pdsch_CodeMapping: Omit

dl_DPCH_InfoPerRL:

fdd:

pCPICH_UsageForChannelEst:mayBeUsed
dpch_FrameOffset:0

secondaryCPICH_Info: Omit

dl_ChannelisationCodeList:

DL_ChannelisationCode:

secondaryScramblingCode:1

sf_AndCodeNumber: (SF512_AndCodeNumber)

sf128:0

scramblingCodeChange:noCodeChange

tpc_CombinationIndex:0
ssdt_CellIdentity: Omit
closedLoopTimingAdjMode: Omit

sccpch_InfoforFACH: Omit

laterNonCriticalExtensions: Omit

specialLI:true

#### RLC_UM_DATA_REQ: rrcConnectionSetup

LLA RLC @ 00:13:39.970

Channel No: 1 Name: CCCH

Message Details:

DL_CCCH_Message:

integrityCheckInfo: Omitted

message:

rrcConnectionSetup:

r3:

rrcConnectionSetup_r3:

initialUE_Identity:

tmsi_and_LAI:

tmsi: 00010001001000100011001101000100

lai:

plmn_Identity:

mcc:

MCC.element: 0

MCC.element: 0

MCC.element: 1

mnc:

MNC.element: 0

MNC.element: 1

lac: 0000000000000001

rrc_TransactionIdentifier: 0

activationTime: Omitted

new_U_RNTI:

srnc_Identity: 000000000001

s_RNTI: 00000000000000000001

new_c_RNTI: Omitted

rrc_StateIndicator: cell_DCH_RRC_StateIndicator [enum=0]

utran_DRX_CycleLengthCoeff: 9

capabilityUpdateRequirement:

ue_RadioCapabilityFDDUpdateRequirement: 1

ue_RadioCapabilityTDDUpdateRequirement: 0

systemSpecificCapUpdateReqList:

SystemSpecificCapUpdateReqList.element: gsm_SystemSpecificCapUpdateReq [enum=0]

srb_InformationSetupList:

SRB_InformationSetupList2.element:

rb_Identity: Omitted

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_UM_RLC_Mode:

transmissionRLC_Discard: Omitted

dl_RLC_Mode:

dl_UM_RLC_Mode: NULL

rb_MappingInfo:

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

dch: 5

logicalChannelIdentity: 1

rlc_SizeList:

configured: NULL

mac_LogicalChannelPriority: 1

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

dch: 10

logicalChannelIdentity: 1

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

rach: NULL

logicalChannelIdentity: 1

rlc_SizeList:

explicitList:

RLC_SizeExplicitList.element:

rlc_SizeIndex: 1

mac_LogicalChannelPriority: 1

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

fach: NULL

logicalChannelIdentity: 1

SRB_InformationSetupList2.element:

rb_Identity: Omitted

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard: dat15_MaxDAT [enum=10]

transmissionWindowSize: tw32_TransmissionWindowSize [enum=3]

timerRST: tr500_TimerRST [enum=9]

max_RST: rst1_MaxRST [enum=0]

pollingInfo:

timerPollProhibit: tpp200_TimerPollProhibit [enum=19]

timerPoll: tp200_TimerPoll [enum=19]

poll_PDU: Omitted

poll_SDU: sdu1_Poll_SDU [enum=0]

lastTransmissionPDU_Poll: 1

lastRetransmissionPDU_Poll: 1

pollWindow: pw99_PollWindow [enum=7]

timerPollPeriodic: Omitted

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery: 1

receivingWindowSize: rw32_ReceivingWindowSize [enum=3]

dl_RLC_StatusInfo:

timerStatusProhibit: tsp200_TimerStatusProhibit [enum=19]

timerEPC: Omitted

missingPDU_Indicator: 1

timerStatusPeriodic: Omitted

rb_MappingInfo:

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

dch: 5

logicalChannelIdentity: 2

rlc_SizeList:

configured: NULL

mac_LogicalChannelPriority: 2

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

dch: 10

logicalChannelIdentity: 2

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

rach: NULL

logicalChannelIdentity: 2

rlc_SizeList:

explicitList:

RLC_SizeExplicitList.element:

rlc_SizeIndex: 1

mac_LogicalChannelPriority: 2

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

fach: NULL

logicalChannelIdentity: 2

SRB_InformationSetupList2.element:

rb_Identity: Omitted

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard: dat15_MaxDAT [enum=10]

transmissionWindowSize: tw32_TransmissionWindowSize [enum=3]

timerRST: tr500_TimerRST [enum=9]

max_RST: rst1_MaxRST [enum=0]

pollingInfo:

timerPollProhibit: tpp200_TimerPollProhibit [enum=19]

timerPoll: tp200_TimerPoll [enum=19]

poll_PDU: Omitted

poll_SDU: sdu1_Poll_SDU [enum=0]

lastTransmissionPDU_Poll: 1

lastRetransmissionPDU_Poll: 1

pollWindow: pw99_PollWindow [enum=7]

timerPollPeriodic: Omitted

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery: 1

receivingWindowSize: rw32_ReceivingWindowSize [enum=3]

dl_RLC_StatusInfo:

timerStatusProhibit: tsp200_TimerStatusProhibit [enum=19]

timerEPC: Omitted

missingPDU_Indicator: 1

timerStatusPeriodic: Omitted

rb_MappingInfo:

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

dch: 5

logicalChannelIdentity: 3

rlc_SizeList:

configured: NULL

mac_LogicalChannelPriority: 3

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

dch: 10

logicalChannelIdentity: 3

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

rach: NULL

logicalChannelIdentity: 3

rlc_SizeList:

explicitList:

RLC_SizeExplicitList.element:

rlc_SizeIndex: 1

mac_LogicalChannelPriority: 3

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

fach: NULL

logicalChannelIdentity: 3

SRB_InformationSetupList2.element:

rb_Identity: Omitted

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard: dat15_MaxDAT [enum=10]

transmissionWindowSize: tw32_TransmissionWindowSize [enum=3]

timerRST: tr500_TimerRST [enum=9]

max_RST: rst1_MaxRST [enum=0]

pollingInfo:

timerPollProhibit: tpp200_TimerPollProhibit [enum=19]

timerPoll: tp200_TimerPoll [enum=19]

poll_PDU: Omitted

poll_SDU: sdu1_Poll_SDU [enum=0]

lastTransmissionPDU_Poll: 1

lastRetransmissionPDU_Poll: 1

pollWindow: pw99_PollWindow [enum=7]

timerPollPeriodic: Omitted

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery: 1

receivingWindowSize: rw32_ReceivingWindowSize [enum=3]

dl_RLC_StatusInfo:

timerStatusProhibit: tsp200_TimerStatusProhibit [enum=19]

timerEPC: Omitted

missingPDU_Indicator: 1

timerStatusPeriodic: Omitted

rb_MappingInfo:

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

dch: 5

logicalChannelIdentity: 4

rlc_SizeList:

configured: NULL

mac_LogicalChannelPriority: 4

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

dch: 10

logicalChannelIdentity: 4

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

rach: NULL

logicalChannelIdentity: 4

rlc_SizeList:

explicitList:

RLC_SizeExplicitList.element:

rlc_SizeIndex: 1

mac_LogicalChannelPriority: 4

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

fach: NULL

logicalChannelIdentity: 4

ul_CommonTransChInfo:

tfc_Subset: Omitted

prach_TFCS: Omitted

modeSpecificInfo:

fdd:

ul_TFCS:

normalTFCI_Signalling:

complete:

ctfcSize:

ctfc2Bit:

ctfc2Bit.noName:

ctfc2: 0

powerOffsetInformation:

gainFactorInformation:

computedGainFactors: 0

powerOffsetPp_m: Omitted

ctfc2Bit.noName:

ctfc2: 1

powerOffsetInformation:

gainFactorInformation:

signalledGainFactors:

modeSpecificInfo:

fdd:

gainFactorBetaC: 11

gainFactorBetaD: 15

referenceTFC_ID: 0

powerOffsetPp_m: Omitted

ul_AddReconfTransChInfoList:

UL_AddReconfTransChInfoList.element:

ul_TransportChannelType: dch_UL_TrCH_Type [enum=0]

transportChannelIdentity: 5

transportFormatSet:

dedicatedTransChTFS:

tti:

tti10:

DedicatedDynamicTF_InfoList.element:

rlc_Size:

bitMode:

sizeType2:

part1: 2

part2: Omitted

numberOfTbSizeList:

numberOfTbSizeList.element:

zero: NULL

numberOfTbSizeList.element:

one: NULL

logicalChannelList:

allSizes: NULL

semistaticTF_Information:

channelCodingType:

convolutional: third_CodingRate [enum=1]

rateMatchingAttribute: 192

crc_Size: crc16_CRC_Size [enum=3]

dl_CommonTransChInfo:

sccpch_TFCS: Omitted

modeSpecificInfo:

fdd:

dl_Parameters:

sameAsUL: NULL

dl_AddReconfTransChInfoList:

DL_AddReconfTransChInfoList.element:

dl_TransportChannelType: dch_DL_TrCH_Type [enum=0]

dl_transportChannelIdentity: 10

tfs_SignallingMode:

sameAsULTrCH:

ul_TransportChannelType: dch_UL_TrCH_Type [enum=0]

ul_TransportChannelIdentity: 5

dch_QualityTarget:

bler_QualityValue: -20

dummy: Omitted

frequencyInfo: Omitted

maxAllowedUL_TX_Power: Omitted

ul_ChannelRequirement:

ul_DPCH_Info:

ul_DPCH_PowerControlInfo:

fdd:

dpcch_PowerOffset: -40

pc_Preamble: 1

sRB_delay: 7

powerControlAlgorithm:

algorithm1: 0

modeSpecificInfo:

fdd:

scramblingCodeType: longSC_ScramblingCodeType [enum=1]

scramblingCode: 0

numberOfDPDCH: Default

spreadingFactor: sf64_SpreadingFactor [enum=4]

tfci_Existence: 1

numberOfFBI_Bits: Omitted

puncturingLimit: pl1_PuncturingLimit [enum=15]

dl_CommonInformation:

dl_DPCH_InfoCommon:

cfnHandling:

initialise:

cfntargetsfnframeoffset: Omitted

modeSpecificInfo:

fdd:

dl_DPCH_PowerControlInfo:

modeSpecificInfo:

fdd:

dpc_Mode: singleTPC_DPC_Mode [enum=0]

powerOffsetPilot_pdpdch: 0

dl_rate_matching_restriction: Omitted

spreadingFactorAndPilot:

sfd128: pb4_PilotBits128 [enum=0]

positionFixedOrFlexible: fixed_PositionFixedOrFlexible [enum=0]

tfci_Existence: 0

modeSpecificInfo:

fdd:

defaultDPCH_OffsetValue: 0

dpch_CompressedModeInfo: Omitted

tx_DiversityMode: noDiversity_TX_DiversityMode [enum=0]

ssdt_Information: Omitted

dl_InformationPerRL_List:

DL_InformationPerRL_List.element:

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode: 100

pdsch_SHO_DCH_Info: Omitted

pdsch_CodeMapping: Omitted

dl_DPCH_InfoPerRL:

fdd:

pCPICH_UsageForChannelEst: mayBeUsed_PCPICH_UsageForChannelEst [enum=0]

dpch_FrameOffset: 0

secondaryCPICH_Info: Omitted

dl_ChannelisationCodeList:

DL_ChannelisationCodeList.element:

secondaryScramblingCode: 1

sf_AndCodeNumber:

sf128: 0

scramblingCodeChange: noCodeChange_ScramblingCodeChange [enum=1]

tpc_CombinationIndex: 0

ssdt_CellIdentity: Omitted

closedLoopTimingAdjMode: Omitted

sccpch_InfoforFACH: Omitted

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]30 E7 22 24 46 68 80 02
[8]01 00 01 00 04 00 00 4D
[16]82 69 3A 10 10 89 0D 42
[24]00 02 81 9E 8E 46 C9 A6
[32]7C 9C 4E 74 20 A5 12 3A
[40]8C 00 15 13 3D 1C 8D 93
[48]4C F9 38 9C E8 42 52 24
[56]B5 28 00 4A 46 7A 39 1B
[64]26 99 F2 71 39 D0 86 B4
[72]49 EA 70 00 D4 C8 00 06
[80]25 2B F0 02 00 08 82 23
[88]BF 66 08 98 95 A5 47 82
[96]00 00 01 3F 90 0A 14 00
[104]02 06 40 00 0C 28 08

#### MAC_DATA_REQ

RLC MAC @ 00:13:40.000

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: CCCH
CFN: 89

Message Details:

RLC PDU size (bits):160
RLC PDU (raw):

[0]3D F8 30 E7 22 24 46 68
[8]80 02 01 00 01 00 04 00
[16]00 4D 82 69

RLC PDU (decoded):

Sequence number:30
Length indicator 0 (octets):124 (the first data octet in this RLC PDU is the first octet of a RLC SDU)
Segment associated with length indicator 0 (0 octets):

Last segment, not associated with any length indicators (18 octets):

[0]30 E7 22 24 46 68 80 02
[8]01 00 01 00 04 00 00 4D
[16]82 69

#### MAC_DATA_REQ

RLC MAC @ 00:13:40.000

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: CCCH
CFN: 89

Message Details:

RLC PDU size (bits):160
RLC PDU (raw):

[0]3E 3A 10 10 89 0D 42 00
[8]02 81 9E 8E 46 C9 A6 7C
[16]9C 4E 74 20

RLC PDU (decoded):

Sequence number:31
Last segment, not associated with any length indicators (19 octets):

[0]3A 10 10 89 0D 42 00 02
[8]81 9E 8E 46 C9 A6 7C 9C
[16]4E 74 20

#### MAC_DATA_REQ

RLC MAC @ 00:13:40.000

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: CCCH
CFN: 89

Message Details:

RLC PDU size (bits):160
RLC PDU (raw):

[0]40 A5 12 3A 8C 00 15 13
[8]3D 1C 8D 93 4C F9 38 9C
[16]E8 42 52 24

RLC PDU (decoded):

Sequence number:32
Last segment, not associated with any length indicators (19 octets):

[0]A5 12 3A 8C 00 15 13 3D
[8]1C 8D 93 4C F9 38 9C E8
[16]42 52 24

#### MAC_DATA_REQ

RLC MAC @ 00:13:40.000

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: CCCH
CFN: 89

Message Details:

RLC PDU size (bits):160
RLC PDU (raw):

[0]42 B5 28 00 4A 46 7A 39
[8]1B 26 99 F2 71 39 D0 86
[16]B4 49 EA 70

RLC PDU (decoded):

Sequence number:33
Last segment, not associated with any length indicators (19 octets):

[0]B5 28 00 4A 46 7A 39 1B
[8]26 99 F2 71 39 D0 86 B4
[16]49 EA 70

#### MAC_DATA_REQ

RLC MAC @ 00:13:40.000

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: CCCH
CFN: 89

Message Details:

RLC PDU size (bits):160
RLC PDU (raw):

[0]44 00 D4 C8 00 06 25 2B
[8]F0 02 00 08 82 23 BF 66
[16]08 98 95 A5

RLC PDU (decoded):

Sequence number:34
Last segment, not associated with any length indicators (19 octets):

[0]00 D4 C8 00 06 25 2B F0
[8]02 00 08 82 23 BF 66 08
[16]98 95 A5

#### MAC_DATA_REQ

RLC MAC @ 00:13:40.000

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: CCCH
CFN: 89

Message Details:

RLC PDU size (bits):160
RLC PDU (raw):

[0]47 23 FE 47 82 00 00 01
[8]3F 90 0A 14 00 02 06 40
[16]00 0C 28 08

RLC PDU (decoded):

Sequence number:35
Length indicator 0 (octets):17
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (17 octets):

[0]47 82 00 00 01 3F 90 0A
[8]14 00 02 06 40 00 0C 28
[16]08
Padding associated with length indicator 1 (0 octets):

#### PHY_DATA_REQ

MAC PHY @ 00:13:40.000

BTS unit: 1:1
Channel No: 0 Name: FACH
CFN: 89

Message Details:

TFI:2
TB set size:336
TB size:168
TB set (raw, each TB word aligned):

[0]40 3D F8 30 E7 22 24 46
[8]68 80 02 01 00 01 00 04
[16]00 00 4D 82 69 00 40 3E
[24]3A 10 10 89 0D 42 00 02
[32]81 9E 8E 46 C9 A6 7C 9C
[40]4E 74 20 00

TB set (decoded):

TB 0:

TCTF:64
MAC SDU (160 bits):

[0]3D F8 30 E7 22 24 46 68
[8]80 02 01 00 01 00 04 00
[16]00 4D 82 69

TB 1:

TCTF:64
MAC SDU (160 bits):

[0]3E 3A 10 10 89 0D 42 00
[8]02 81 9E 8E 46 C9 A6 7C
[16]9C 4E 74 20

#### PHY_DATA_REQ

MAC PHY @ 00:13:40.010

BTS unit: 1:1
Channel No: 0 Name: FACH
CFN: 90

Message Details:

TFI:2
TB set size:336
TB size:168
TB set (raw, each TB word aligned):

[0]40 40 A5 12 3A 8C 00 15
[8]13 3D 1C 8D 93 4C F9 38
[16]9C E8 42 52 24 00 40 42
[24]B5 28 00 4A 46 7A 39 1B
[32]26 99 F2 71 39 D0 86 B4
[40]49 EA 70 00

TB set (decoded):

TB 0:

TCTF:64
MAC SDU (160 bits):

[0]40 A5 12 3A 8C 00 15 13
[8]3D 1C 8D 93 4C F9 38 9C
[16]E8 42 52 24

TB 1:

TCTF:64
MAC SDU (160 bits):

[0]42 B5 28 00 4A 46 7A 39
[8]1B 26 99 F2 71 39 D0 86
[16]B4 49 EA 70

#### PHY_DATA_REQ

MAC PHY @ 00:13:40.020

BTS unit: 1:1
Channel No: 0 Name: FACH
CFN: 91

Message Details:

TFI:2
TB set size:336
TB size:168
TB set (raw, each TB word aligned):

[0]40 44 00 D4 C8 00 06 25
[8]2B F0 02 00 08 82 23 BF
[16]66 08 98 95 A5 00 40 47
[24]23 FE 47 82 00 00 01 3F
[32]90 0A 14 00 02 06 40 00
[40]0C 28 08 00

TB set (decoded):

TB 0:

TCTF:64
MAC SDU (160 bits):

[0]44 00 D4 C8 00 06 25 2B
[8]F0 02 00 08 82 23 BF 66
[16]08 98 95 A5

TB 1:

TCTF:64
MAC SDU (160 bits):

[0]47 23 FE 47 82 00 00 01
[8]3F 90 0A 14 00 02 06 40
[16]00 0C 28 08

#### CPHY_SYNC_IND

PHY RRC @ 00:13:40.230

BTS unit: 1:1
Channel No: 0 Name: U_DPCH
CFN: 112

Message Details:

#### PHY_DATA_IND

PHY MAC @ 00:13:40.400

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 109

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 00 04 B0 C0 00 08 00
[8]00 51 1B 8D D0 6A 4C 66
[16]88 A2 C0 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 00 4B 0C 00 00 80 00
[8]05 11 B8 DD 06 A4 C6 68
[16]8A 2C

#### MAC_DATA_IND

MAC RLC @ 00:13:40.400

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 109

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 00 4B 0C 00 00 80 00
[8]05 11 B8 DD 06 A4 C6 68
[16]8A 2C

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:0
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]4B 0C 00 00 80 00 05 11
[8]B8 DD 06 A4 C6 68 8A 2C

#### PHY_DATA_IND

PHY MAC @ 00:13:40.410

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 110

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 00 88 30 34 80 01 80
[8]01 18 FC FC 0C C0 D5 C6
[16]28 48 C0 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 08 83 03 48 00 18 00
[8]11 8F CF C0 CC 0D 5C 62
[16]84 8C

#### MAC_DATA_IND

MAC RLC @ 00:13:40.410

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 110

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 08 83 03 48 00 18 00
[8]11 8F CF C0 CC 0D 5C 62
[16]84 8C

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:1
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]83 03 48 00 18 00 11 8F
[8]CF C0 CC 0D 5C 62 84 8C

#### PHY_DATA_IND

PHY MAC @ 00:13:40.420

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 111

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 01 50 BF E0 28 99 01
[8]00 05 55 55 55 55 55 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 15 0B FE 02 89 90 10
[8]00 55 55 55 55 55 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:13:40.420

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 111

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 15 0B FE 02 89 90 10
[8]00 55 55 55 55 55 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:2
Polling bit:1 (request a status report)
Length indicator 0 (octets):5
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (5 octets):

[0]02 89 90 10 00
Padding associated with length indicator 1 (9 octets):

[0]55 55 55 55 55 55 55 55
[8]55

#### MAC_DATA_REQ

RLC MAC @ 00:13:40.430

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 132

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:3

#### PHY_DATA_REQ

MAC PHY @ 00:13:40.430

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 132

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]10 20 03 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:13:40.430

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 112

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 00 01 50 08 80 04 02
[8]80 AB 82 FA 08 91 19 A2
[16]20 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 00 15 00 88 00 40 28
[8]0A B8 2F A0 89 11 9A 22
[16]00 00

#### MAC_DATA_IND

MAC RLC @ 00:13:40.430

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 112

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 00 15 00 88 00 40 28
[8]0A B8 2F A0 89 11 9A 22
[16]00 00

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:0
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]15 00 88 00 40 28 0A B8
[8]2F A0 89 11 9A 22 00 00

#### PHY_DATA_IND

PHY MAC @ 00:13:40.440

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 113

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 00 D0 3F E4 05 55 55
[8]55 55 55 55 55 55 55 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 0D 03 FE 40 55 55 55
[8]55 55 55 55 55 55 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:13:40.440

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 113

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 0D 03 FE 40 55 55 55
[8]55 55 55 55 55 55 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:1
Polling bit:1 (request a status report)
Length indicator 0 (octets):1
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (1 octets):

[0]40
Padding associated with length indicator 1 (13 octets):

[0]55 55 55 55 55 55 55 55
[8]55 55 55 55 55

#### RLC_AM_DATA_IND: rrcConnectionSetupComplete

RLC LLA @ 00:13:40.440

Channel No: 2 Name: DCCH

Message Details:

UL_DCCH_Message:

integrityCheckInfo: Omitted

message:

rrcConnectionSetupComplete:

rrc_TransactionIdentifier: 0

startList:

STARTList.element:

cn_DomainIdentity: ps_domain_CN_DomainIdentity [enum=1]

start_Value: 00000000000000000010

STARTList.element:

cn_DomainIdentity: cs_domain_CN_DomainIdentity [enum=0]

start_Value: 00000000000000000010

ue_RadioAccessCapability:

accessStratumReleaseIndicator: r99_AccessStratumReleaseIndicator [enum=0]

pdcp_Capability:

losslessSRNS_RelocationSupport: 0

supportForRfc2507:

notSupported: NULL

rlc_Capability:

totalRLC_AM_BufferSize: kb50_TotalRLC_AM_BufferSize [enum=2]

maximumRLC_WindowSize: mws2047_MaximumRLC_WindowSize [enum=0]

maximumAM_EntityNumber: am6_MaximumAM_EntityNumberRLC_Cap [enum=3]

transportChannelCapability:

dl_TransChCapability:

maxNoBitsReceived: b8960_MaxNoBits [enum=7]

maxConvCodeBitsReceived: b1280_MaxNoBits [enum=1]

turboDecodingSupport:

supported: b8960_MaxNoBits [enum=7]

maxSimultaneousTransChs: e8_MaxSimultaneousTransChsDL [enum=1]

maxSimultaneousCCTrCH_Count: 1

maxReceivedTransportBlocks: tb32_MaxTransportBlocksDL [enum=3]

maxNumberOfTFC: tfc128_MaxNumberOfTFC_DL [enum=5]

maxNumberOfTF: tf64_MaxNumberOfTF [enum=1]

ul_TransChCapability:

maxNoBitsTransmitted: b3840_MaxNoBits [enum=3]

maxConvCodeBitsTransmitted: b1280_MaxNoBits [enum=1]

turboEncodingSupport:

supported: b3840_MaxNoBits [enum=3]

maxSimultaneousTransChs: e8_MaxSimultaneousTransChsUL [enum=2]

modeSpecificInfo:

fdd: NULL

maxTransmittedBlocks: tb32_MaxTransportBlocksUL [enum=4]

maxNumberOfTFC: tfc64_MaxNumberOfTFC_UL [enum=5]

maxNumberOfTF: tf32_MaxNumberOfTF [enum=0]

rf_Capability:

fddRF_Capability:

ue_PowerClass: 4

txRxFrequencySeparation: mhz190_TxRxFrequencySeparation [enum=0]

tddRF_Capability: Omitted

physicalChannelCapability:

fddPhysChCapability:

downlinkPhysChCapability:

maxNoDPCH_PDSCH_Codes: 1

maxNoPhysChBitsReceived: b9600_MaxNoPhysChBitsReceived [enum=6]

supportForSF_512: 0

supportOfPDSCH: 0

simultaneousSCCPCH_DPCH_Reception:

notSupported: NULL

uplinkPhysChCapability:

maxNoDPDCH_BitsTransmitted: b4800_MaxNoDPDCH_BitsTransmitted [enum=3]

supportOfPCPCH: 0

tddPhysChCapability: Omitted

ue_MultiModeRAT_Capability:

multiRAT_CapabilityList:

supportOfGSM: 1

supportOfMulticarrier: 0

multiModeCapability: fdd_MultiModeCapability [enum=1]

securityCapability:

cipheringAlgorithmCap: 0000000000000011

integrityProtectionAlgorithmCap: 0000000000000010

ue_positioning_Capability:

standaloneLocMethodsSupported: 0

ue_BasedOTDOA_Supported: 0

networkAssistedGPS_Supported: noNetworkAssistedGPS_NetworkAssistedGPS_Supported [enum=3]

supportForUE_GPS_TimingOfCellFrames: 0

supportForIPDL: 0

measurementCapability:

downlinkCompressedMode:

fdd_Measurements: 1

tdd_Measurements: Omitted

gsm_Measurements:

gsm900: 1

dcs1800: 1

gsm1900: 1

multiCarrierMeasurements: 0

uplinkCompressedMode:

fdd_Measurements: 1

tdd_Measurements: Omitted

gsm_Measurements:

gsm900: 1

dcs1800: 1

gsm1900: 1

multiCarrierMeasurements: 0

ue_RATSpecificCapability:

InterRAT_UE_RadioAccessCapabilityList.element:

gsm:

gsm_Classmark2: 33035718A1

gsm_Classmark3: 60144C8080

v370NonCriticalExtensions: Omitted

Layer 3 SDU:

[0]4B 0C 00 00 80 00 05 11
[8]B8 DD 06 A4 C6 68 8A 2C
[16]83 03 48 00 18 00 11 8F
[24]CF C0 CC 0D 5C 62 84 8C
[32]02 89 90 10 00

#### RLC_AM_DATA_IND

LLA RRC @ 00:13:40.440

Channel ID: Rb2
Cell ID: -1

Message Details:

RLC_AM_DATA_IND:

cellId:-1

routingInfo:

rB_Identity:2

integrityResult:

integrityUsed (IntegrityStatus):i_pass

aM_message:

uL_DCCH_Message:

integrityCheckInfo: Omit

message: (UL_DCCH_MessageType)

rrcConnectionSetupComplete:

rrc_TransactionIdentifier:0

startList:

STARTSingle:

cn_DomainIdentity:ps_domain
start_Value:00000000000000000010

STARTSingle:

cn_DomainIdentity:cs_domain
start_Value:00000000000000000010

ue_RadioAccessCapability:

accessStratumReleaseIndicator:r99

pdcp_Capability:

losslessSRNS_RelocationSupport:false

supportForRfc2507:

notSupported:

rlc_Capability:

totalRLC_AM_BufferSize:kb50
maximumRLC_WindowSize:mws2047
maximumAM_EntityNumber (MaximumAM_EntityNumberRLC_Cap):am6

transportChannelCapability:

dl_TransChCapability:

maxNoBitsReceived (MaxNoBits):b8960
maxConvCodeBitsReceived (MaxNoBits):b1280

turboDecodingSupport: (TurboSupport)

supported (MaxNoBits):b8960

maxSimultaneousTransChs (MaxSimultaneousTransChsDL):e8
maxSimultaneousCCTrCH_Count:1
maxReceivedTransportBlocks (MaxTransportBlocksDL):tb32
maxNumberOfTFC (MaxNumberOfTFC_DL):tfc128
maxNumberOfTF:tf64

ul_TransChCapability:

maxNoBitsTransmitted (MaxNoBits):b3840
maxConvCodeBitsTransmitted (MaxNoBits):b1280

turboEncodingSupport: (TurboSupport)

supported (MaxNoBits):b3840

maxSimultaneousTransChs (MaxSimultaneousTransChsUL):e8

modeSpecificInfo:

fdd:

maxTransmittedBlocks (MaxTransportBlocksUL):tb32
maxNumberOfTFC (MaxNumberOfTFC_UL):tfc64
maxNumberOfTF:tf32

rf_Capability:

fddRF_Capability:

ue_PowerClass:4
txRxFrequencySeparation:mhz190

tddRF_Capability: Omit

physicalChannelCapability:

fddPhysChCapability:

downlinkPhysChCapability: (DL_PhysChCapabilityFDD)

maxNoDPCH_PDSCH_Codes:1
maxNoPhysChBitsReceived:b9600
supportForSF_512:false
supportOfPDSCH:false

simultaneousSCCPCH_DPCH_Reception:

notSupported:

uplinkPhysChCapability: (UL_PhysChCapabilityFDD)

maxNoDPDCH_BitsTransmitted:b4800
supportOfPCPCH:false

tddPhysChCapability: Omit

ue_MultiModeRAT_Capability:

multiRAT_CapabilityList: (MultiRAT_Capability)

supportOfGSM:true
supportOfMulticarrier:false

multiModeCapability:fdd

securityCapability:

cipheringAlgorithmCap:0000000000000011
integrityProtectionAlgorithmCap:0000000000000010

ue_positioning_Capability:

standaloneLocMethodsSupported:false
ue_BasedOTDOA_Supported:false
networkAssistedGPS_Supported:noNetworkAssistedGPS
supportForUE_GPS_TimingOfCellFrames:false
supportForIPDL:false

measurementCapability:

downlinkCompressedMode: (CompressedModeMeasCapability)

fdd_Measurements:true
tdd_Measurements: Omit

gsm_Measurements:

gsm900:true
dcs1800:true
gsm1900:true

multiCarrierMeasurements:false

uplinkCompressedMode: (CompressedModeMeasCapability)

fdd_Measurements:true
tdd_Measurements: Omit

gsm_Measurements:

gsm900:true
dcs1800:true
gsm1900:true

multiCarrierMeasurements:false

ue_RATSpecificCapability: (InterRAT_UE_RadioAccessCapabilityList)

InterRAT_UE_RadioAccessCapability:

gsm:

gsm_Classmark2:

[0]33 03 57 18 A1
gsm_Classmark3:

[0]60 14 4C 80 80

v370NonCriticalExtensions: Omit

#### RLC_AM_DATA_IND: initialDirectTransfer

RLC RRC @ 00:13:40.450

Channel No: 3 Name: DCCH

Message Details:

UL_DCCH_Message:

integrityCheckInfo: Omitted

message:

initialDirectTransfer:

cn_DomainIdentity: cs_domain_CN_DomainIdentity [enum=0]

intraDomainNasNodeSelector:

version:

release99:

cn_Type:

gsm_Map_IDNNS:

routingbasis:

localPTMSI:

routingparameter: 0010001000

enteredparameter: 0

nas_Message: 05015705F411223344

measuredResultsOnRACH: Omitted

v3a0NonCriticalExtensions:

initialDirectTransfer_v3a0ext:

start_Value: 00000000000000000010

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]15 00 88 00 40 28 0A B8
[8]2F A0 89 11 9A 22 00 00
[16]40

#### RRC_DATA_IND: mm:imsiDetachIndication

RRC NAS @ 00:13:40.450

Cell ID: -1

Message Details:

IMSIDETACHINDICATION:

skipIndicator: 0000

mMProtocolDiscriminator: 0101

msgType: 00000001

mSClsmk1:

spare1: 0

revLvl: 10

eSIND: 1

a5_1: 0

rFPwrCap: 111

mobileId:

iel: 05

iDigit1: 1111

oddEvenInd: 0

typeOfId: 100

otherDigits: 11223344

#### MAC_DATA_REQ

RLC MAC @ 00:13:40.450

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 134

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 20 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:2

#### PHY_DATA_REQ

MAC PHY @ 00:13:40.450

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 134

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 02 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 20 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:13:40.630

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 132

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 01 50 BF E0 28 99 01
[8]00 05 55 55 55 55 55 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 15 0B FE 02 89 90 10
[8]00 55 55 55 55 55 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:13:40.630

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 132

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 15 0B FE 02 89 90 10
[8]00 55 55 55 55 55 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:2
Polling bit:1 (request a status report)
Length indicator 0 (octets):5
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (5 octets):

[0]02 89 90 10 00
Padding associated with length indicator 1 (9 octets):

[0]55 55 55 55 55 55 55 55
[8]55

#### MAC_DATA_REQ

RLC MAC @ 00:13:40.640

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 153

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:3

#### PHY_DATA_REQ

MAC PHY @ 00:13:40.640

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 153

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]10 20 03 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:13:40.650

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 134

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 00 D0 3F E4 05 55 55
[8]55 55 55 55 55 55 55 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 0D 03 FE 40 55 55 55
[8]55 55 55 55 55 55 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:13:40.650

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 134

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 0D 03 FE 40 55 55 55
[8]55 55 55 55 55 55 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:1
Polling bit:1 (request a status report)
Length indicator 0 (octets):1
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (1 octets):

[0]40
Padding associated with length indicator 1 (13 octets):

[0]55 55 55 55 55 55 55 55
[8]55 55 55 55 55

#### MAC_DATA_REQ

RLC MAC @ 00:13:40.660

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 155

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 20 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:2

#### PHY_DATA_REQ

MAC PHY @ 00:13:40.660

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 155

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 02 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 20 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### RLC_UM_DATA_REQ

RRC LLA @ 00:13:41.470

Channel ID: Rb1
Cell ID: -1

Message Details:

RLC_UM_DATA_REQ:

cellId:-1

routingInfo:

rB_Identity:1

uM_message:

dL_DCCH_Message:

integrityCheckInfo: Omit

message: (DL_DCCH_MessageType)

rrcConnectionRelease:

r3:

rrcConnectionRelease_r3: (RRCConnectionRelease_r3_IEs)

rrc_TransactionIdentifier:0
n_308:1
releaseCause:normalEvent

rplmn_information: Omit

laterNonCriticalExtensions: Omit

specialLI:false

#### RLC_UM_DATA_REQ: rrcConnectionRelease

LLA RLC @ 00:13:41.470

Channel No: 1 Name: DCCH

Message Details:

DL_DCCH_Message:

integrityCheckInfo: Omitted

message:

rrcConnectionRelease:

r3:

rrcConnectionRelease_r3:

rrc_TransactionIdentifier: 0

n_308: 1

releaseCause: normalEvent_ReleaseCause [enum=0]

rplmn_information: Omitted

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]3C 80 00

#### MAC_DATA_REQ

RLC MAC @ 00:13:41.470

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 236

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]01 07 FE 3C 80 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

Sequence number:0
Length indicator 0 (octets):3
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (3 octets):

[0]3C 80 00
Padding associated with length indicator 1 (12 octets):

[0]00 00 00 00 00 00 00 00
[8]00 00 00 00

#### PHY_DATA_REQ

MAC PHY @ 00:13:41.470

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 236

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]00 10 7F E3 C8 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:0
MAC SDU (144 bits):

[0]01 07 FE 3C 80 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:13:41.710

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 240

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]00 10 5F E4 40 05 55 55
[8]55 55 55 55 55 55 55 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:0
MAC SDU (144 bits):

[0]01 05 FE 44 00 55 55 55
[8]55 55 55 55 55 55 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:13:41.710

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 240

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]01 05 FE 44 00 55 55 55
[8]55 55 55 55 55 55 55 55
[16]55 55

RLC PDU (decoded):

Sequence number:0
Length indicator 0 (octets):2
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (2 octets):

[0]44 00
Padding associated with length indicator 1 (13 octets):

[0]55 55 55 55 55 55 55 55
[8]55 55 55 55 55

#### RLC_UM_DATA_IND: rrcConnectionReleaseComplete

RLC LLA @ 00:13:41.740

Channel No: 1 Name: DCCH

Message Details:

UL_DCCH_Message:

integrityCheckInfo: Omitted

message:

rrcConnectionReleaseComplete:

rrc_TransactionIdentifier: 0

errorIndication: Omitted

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]44 00

#### RLC_UM_DATA_IND

LLA RRC @ 00:13:41.740

Channel ID: Rb1
Cell ID: -1

Message Details:

RLC_UM_DATA_IND:

cellId:-1

routingInfo:

rB_Identity:1

integrityResult:

integrityUsed (IntegrityStatus):i_pass

uM_message:

uL_DCCH_Message:

integrityCheckInfo: Omit

message: (UL_DCCH_MessageType)

rrcConnectionReleaseComplete:

rrc_TransactionIdentifier:0

errorIndication: (FailureCauseWithProtErr) Omit

laterNonCriticalExtensions: Omit

#### PHY_DATA_IND

PHY MAC @ 00:13:41.870

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 0

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]00 30 5F E4 40 05 55 55
[8]55 55 55 55 55 55 55 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:0
MAC SDU (144 bits):

[0]03 05 FE 44 00 55 55 55
[8]55 55 55 55 55 55 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:13:41.870

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 0

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]03 05 FE 44 00 55 55 55
[8]55 55 55 55 55 55 55 55
[16]55 55

RLC PDU (decoded):

Sequence number:1
Length indicator 0 (octets):2
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (2 octets):

[0]44 00
Padding associated with length indicator 1 (13 octets):

[0]55 55 55 55 55 55 55 55
[8]55 55 55 55 55

#### CRLC UM Channel Release REQ

LLA RLC @ 00:13:41.910

BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 24

Message Details:

#### CRLC UM Channel Release CNF

RLC LLA @ 00:13:41.910

BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 24

Message Details:

#### RLC_UM_DATA_IND: rrcConnectionReleaseComplete

RLC LLA @ 00:13:41.910

Channel No: 1 Name: DCCH

Message Details:

UL_DCCH_Message:

integrityCheckInfo: Omitted

message:

rrcConnectionReleaseComplete:

rrc_TransactionIdentifier: 0

errorIndication: Omitted

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]44 00

#### RLC_UM_DATA_IND

LLA RRC @ 00:13:41.910

Channel ID: Rb1
Cell ID: -1

Message Details:

RLC_UM_DATA_IND:

cellId:-1

routingInfo:

rB_Identity:1

integrityResult:

integrityUsed (IntegrityStatus):i_pass

uM_message:

uL_DCCH_Message:

integrityCheckInfo: Omit

message: (UL_DCCH_MessageType)

rrcConnectionReleaseComplete:

rrc_TransactionIdentifier:0

errorIndication: (FailureCauseWithProtErr) Omit

laterNonCriticalExtensions: Omit

#### CRLC_Config_REQ

RRC LLA @ 00:13:41.910

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:1

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC AM Channel Release REQ

LLA RLC @ 00:13:41.920

BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 25

Message Details:

#### CRLC AM Channel Release CNF

RLC LLA @ 00:13:41.920

BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 25

Message Details:

#### CPHY_OUTSYNC_IND

PHY RRC @ 00:13:41.930

BTS unit: 1:1
Channel No: 0 Name: U_DPCH
CFN: 26

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:13:41.930

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:1

#### CRLC_Config_REQ

RRC LLA @ 00:13:41.930

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:2

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC_Config_CNF

LLA RRC @ 00:13:41.940

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:2

#### CRLC_Config_REQ

RRC LLA @ 00:13:41.940

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:3

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC AM Channel Release REQ

LLA RLC @ 00:13:41.940

BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 27

Message Details:

#### CRLC AM Channel Release CNF

RLC LLA @ 00:13:41.940

BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 27

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:13:41.960

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:3

#### CRLC_Config_REQ

RRC LLA @ 00:13:41.960

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:4

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC AM Channel Release REQ

LLA RLC @ 00:13:41.960

BTS unit: 1:1
Channel No: 4 Name: DCCH
CFN: 29

Message Details:

#### CRLC AM Channel Release CNF

RLC LLA @ 00:13:41.960

BTS unit: 1:1
Channel No: 4 Name: DCCH
CFN: 29

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:13:41.970

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:4

#### CRLC_Config_REQ

RRC LLA @ 00:13:41.970

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:1

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode)

dl_UM_RLC_Mode:

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):136

dl_RLCModeInfo: (UL_RLC_Mode)

ul_UM_RLC_Mode:

transmissionRLC_Discard:

timerBasedNoExplicit (NoExplicitDiscard):dt100

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity):1
dLlogicalChannelIdentity (LogicalChannelIdentity):1
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC UM Channel Establish REQ

LLA RLC @ 00:13:41.970

BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 30

Message Details:

Configuration Parameters:

PU Size In Bits:136

#### CRLC UM Channel Establish CNF

RLC LLA @ 00:13:41.970

BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 30

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:13:41.990

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:1

#### CRLC_Config_REQ

RRC LLA @ 00:13:41.990

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:2

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode)

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):128

dl_RLCModeInfo: (UL_RLC_Mode)

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity):2
dLlogicalChannelIdentity (LogicalChannelIdentity):2
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC AM Channel Establish REQ

LLA RLC @ 00:13:41.990

BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 32

Message Details:

Configuration Parameters:

PU Size In Bits:128

Timer Parameters:

Poll (ms):200
Poll Prohibit (ms):0
EPC (ms):0
Discard (ms):0
Poll Periodic (ms):0
Status Prohibit (ms):0
Status Periodic (ms):0
Reset (ms):500
MRW (ms):0

Protocol Parameters:

Max Dat:15
Poll PU:0
Poll SDU:1
Poll Window:99
Max Reset:1
Tx Window Size:32
Rx Window Size:32
Max MRW:0
SDU Discard Mode:No discard

Polling Triggers:

Last PU In Buffer:On
Last PU In Retransmission Buffer:On
Poll Timer:On
Every Poll-PU PU:Off
Every Poll-SDU SDU:On
Poll-Window Percent Of Transmission Buffer:On
Timer Based:Off

Status Triggers:

Missing PU:On
Timer Based:Off
EPC Mechanism:Off

#### CRLC AM Channel Establish CNF

RLC LLA @ 00:13:41.990

BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 32

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:13:42.000

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:2

#### CRLC_Config_REQ

RRC LLA @ 00:13:42.000

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:3

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode)

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):128

dl_RLCModeInfo: (UL_RLC_Mode)

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity):3
dLlogicalChannelIdentity (LogicalChannelIdentity):3
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC AM Channel Establish REQ

LLA RLC @ 00:13:42.000

BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 33

Message Details:

Configuration Parameters:

PU Size In Bits:128

Timer Parameters:

Poll (ms):200
Poll Prohibit (ms):0
EPC (ms):0
Discard (ms):0
Poll Periodic (ms):0
Status Prohibit (ms):0
Status Periodic (ms):0
Reset (ms):500
MRW (ms):0

Protocol Parameters:

Max Dat:15
Poll PU:0
Poll SDU:1
Poll Window:99
Max Reset:1
Tx Window Size:32
Rx Window Size:32
Max MRW:0
SDU Discard Mode:No discard

Polling Triggers:

Last PU In Buffer:On
Last PU In Retransmission Buffer:On
Poll Timer:On
Every Poll-PU PU:Off
Every Poll-SDU SDU:On
Poll-Window Percent Of Transmission Buffer:On
Timer Based:Off

Status Triggers:

Missing PU:On
Timer Based:Off
EPC Mechanism:Off

#### CRLC AM Channel Establish CNF

RLC LLA @ 00:13:42.000

BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 33

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:13:42.020

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:3

#### CRLC_Config_REQ

RRC LLA @ 00:13:42.020

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:4

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode)

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):128

dl_RLCModeInfo: (UL_RLC_Mode)

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity):4
dLlogicalChannelIdentity (LogicalChannelIdentity):4
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC AM Channel Establish REQ

LLA RLC @ 00:13:42.020

BTS unit: 1:1
Channel No: 4 Name: DCCH
CFN: 35

Message Details:

Configuration Parameters:

PU Size In Bits:128

Timer Parameters:

Poll (ms):200
Poll Prohibit (ms):0
EPC (ms):0
Discard (ms):0
Poll Periodic (ms):0
Status Prohibit (ms):0
Status Periodic (ms):0
Reset (ms):500
MRW (ms):0

Protocol Parameters:

Max Dat:15
Poll PU:0
Poll SDU:1
Poll Window:99
Max Reset:1
Tx Window Size:32
Rx Window Size:32
Max MRW:0
SDU Discard Mode:No discard

Polling Triggers:

Last PU In Buffer:On
Last PU In Retransmission Buffer:On
Poll Timer:On
Every Poll-PU PU:Off
Every Poll-SDU SDU:On
Poll-Window Percent Of Transmission Buffer:On
Timer Based:Off

Status Triggers:

Missing PU:On
Timer Based:Off
EPC Mechanism:Off

#### CRLC AM Channel Establish CNF

RLC LLA @ 00:13:42.020

BTS unit: 1:1
Channel No: 4 Name: DCCH
CFN: 35

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:13:42.040

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:4

#### CRLC_Config_REQ

RRC LLA @ 00:13:44.110

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:1

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC UM Channel Release REQ

LLA RLC @ 00:13:44.110

BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 244

Message Details:

#### CRLC UM Channel Release CNF

RLC LLA @ 00:13:44.110

BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 244

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:13:44.130

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:1

#### CRLC_Config_REQ

RRC LLA @ 00:13:44.130

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:2

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC AM Channel Release REQ

LLA RLC @ 00:13:44.130

BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 246

Message Details:

#### CRLC AM Channel Release CNF

RLC LLA @ 00:13:44.130

BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 246

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:13:44.140

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:2

#### CRLC_Config_REQ

RRC LLA @ 00:13:44.140

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:3

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC AM Channel Release REQ

LLA RLC @ 00:13:44.150

BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 248

Message Details:

#### CRLC AM Channel Release CNF

RLC LLA @ 00:13:44.150

BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 248

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:13:44.160

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:3

#### CRLC_Config_REQ

RRC LLA @ 00:13:44.160

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:4

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC AM Channel Release REQ

LLA RLC @ 00:13:44.160

BTS unit: 1:1
Channel No: 4 Name: DCCH
CFN: 249

Message Details:

#### CRLC AM Channel Release CNF

RLC LLA @ 00:13:44.160

BTS unit: 1:1
Channel No: 4 Name: DCCH
CFN: 249

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:13:44.180

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:4

#### CMAC_Config_REQ

RRC LLA @ 00:13:44.180

Channel ID: DL-DPCH#1
Cell ID: -1

Message Details:

CMAC_Config_REQ:

cellId:-1

routingInfo:

physicalChannelIdentity:26

ratType:fdd

configMessage:

release:

#### CMAC Configuration REQ

LLA MAC @ 00:13:44.180

BTS unit: 1:1
Channel No: 0 Name: D_DPCH
CFN: 251

Message Details:

Configuration Parameters:

Number Of Transport Channels:0
Active Flag:0

Transport Format Combination Set:

Number Of Transport Format Combinations:0

#### CMAC Configuration CNF

MAC LLA @ 00:13:44.180

BTS unit: 1:1
Channel No: 0 Name: D_DPCH
CFN: 251

Message Details:

#### CMAC_Config_CNF

LLA RRC @ 00:13:44.210

Channel ID: DL-DPCH#1
Cell ID: -1

Message Details:

CMAC_Config_CNF:

cellId:-1

routingInfo:

physicalChannelIdentity:26

#### CMAC_Config_REQ

RRC LLA @ 00:13:44.210

Channel ID: UL-DPCH#1
Cell ID: -1

Message Details:

CMAC_Config_REQ:

cellId:-1

routingInfo:

physicalChannelIdentity:20

ratType:fdd

configMessage:

release:

#### CMAC Configuration REQ

LLA MAC @ 00:13:44.210

BTS unit: 1:1
Channel No: 0 Name: U_DPCH
CFN: 254

Message Details:

Configuration Parameters:

Number Of Transport Channels:0
Active Flag:0

Transport Format Combination Set:

Number Of Transport Format Combinations:0

#### CMAC Configuration CNF

MAC LLA @ 00:13:44.210

BTS unit: 1:1
Channel No: 0 Name: U_DPCH
CFN: 254

Message Details:

#### CMAC_Config_CNF

LLA RRC @ 00:13:44.220

Channel ID: UL-DPCH#1
Cell ID: -1

Message Details:

CMAC_Config_CNF:

cellId:-1

routingInfo:

physicalChannelIdentity:20

#### CPHY_TrCH_Release_REQ

RRC LLA @ 00:13:44.220

Channel ID: DL-DPCH#1
Cell ID: 0

Message Details:

CPHY_TrCH_Release_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:26

trchConfigType:

dch:normal

#### CPHY Transport Channel Release REQ

LLA PHY @ 00:13:44.220

BTS unit: 1:1
Channel No: 0 Name: D_DPCH
CFN: 255

Message Details:

#### CPHY Transport Channel Release CNF

PHY LLA @ 00:13:44.220

BTS unit: 1:1
Channel No: 0 Name: D_DPCH
CFN: 255

Message Details:

#### CPHY_TrCH_Release_CNF

LLA RRC @ 00:13:44.240

Channel ID: DL-DPCH#1
Cell ID: 0

Message Details:

CPHY_TrCH_Release_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:26

#### CPHY_TrCH_Release_REQ

RRC LLA @ 00:13:44.240

Channel ID: UL-DPCH#1
Cell ID: 0

Message Details:

CPHY_TrCH_Release_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:20

trchConfigType:

dch:normal

#### CPHY Transport Channel Release REQ

LLA PHY @ 00:13:44.240

BTS unit: 1:1
Channel No: 0 Name: U_DPCH
CFN: 1

Message Details:

#### CPHY Transport Channel Release CNF

PHY LLA @ 00:13:44.240

BTS unit: 1:1
Channel No: 0 Name: U_DPCH
CFN: 1

Message Details:

#### CPHY_TrCH_Release_CNF

LLA RRC @ 00:13:44.250

Channel ID: UL-DPCH#1
Cell ID: 0

Message Details:

CPHY_TrCH_Release_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:20

#### CPHY_RL_Release_REQ

RRC LLA @ 00:13:44.250

Channel ID: DL-DPCH#1
Cell ID: 0

Message Details:

CPHY_RL_Release_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:26

#### CPHY Radio Link Release REQ

LLA PHY @ 00:13:44.250

BTS unit: 1:1
Channel No: 0 Name: D_DPCH
CFN: 2

Message Details:

#### CPHY Radio Link Release CNF

PHY LLA @ 00:13:44.250

BTS unit: 1:1
Channel No: 0 Name: D_DPCH
CFN: 2

Message Details:

#### CPHY_RL_Release_CNF

LLA RRC @ 00:13:44.270

Channel ID: DL-DPCH#1
Cell ID: 0

Message Details:

CPHY_RL_Release_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:26

#### CPHY_RL_Release_REQ

RRC LLA @ 00:13:44.270

Channel ID: UL-DPCH#1
Cell ID: 0

Message Details:

CPHY_RL_Release_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:20

#### CPHY Radio Link Release REQ

LLA PHY @ 00:13:44.270

BTS unit: 1:1
Channel No: 0 Name: U_DPCH
CFN: 4

Message Details:

#### CPHY Radio Link Release CNF

PHY LLA @ 00:13:44.270

BTS unit: 1:1
Channel No: 0 Name: U_DPCH
CFN: 4

Message Details:

#### CRLC UM Channel Release REQ

LLA RLC @ 00:13:44.280

BTS unit: 1:1
Channel No: 1 Name: CCCH
CFN: 5

Message Details:

#### CRLC UM Channel Release CNF

RLC LLA @ 00:13:44.280

BTS unit: 1:1
Channel No: 1 Name: CCCH
CFN: 5

Message Details:

#### CPHY_RL_Release_CNF

LLA RRC @ 00:13:44.290

Channel ID: UL-DPCH#1
Cell ID: 0

Message Details:

CPHY_RL_Release_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:20

#### CRLC_Config_REQ

RRC LLA @ 00:13:44.290

Channel ID: Rb0
Cell ID: 0

Message Details:

CRLC_Config_REQ:

cellId:0

routingInfo:

rB_Identity:0

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC_Config_CNF

LLA RRC @ 00:13:44.300

Channel ID: Rb0
Cell ID: 0

Message Details:

CRLC_Config_CNF:

cellId:0

routingInfo:

rB_Identity:0

#### CMAC_Config_REQ

RRC LLA @ 00:13:44.300

Channel ID: PRACH#1
Cell ID: 0

Message Details:

CMAC_Config_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:8

ratType:fdd

configMessage:

release:

#### CMAC Configuration REQ

LLA MAC @ 00:13:44.300

BTS unit: 1:1
Channel No: 0 Name: PRACH
CFN: 7

Message Details:

Configuration Parameters:

Number Of Transport Channels:0
Active Flag:0

Transport Format Combination Set:

Number Of Transport Format Combinations:0

#### CMAC Configuration CNF

MAC LLA @ 00:13:44.300

BTS unit: 1:1
Channel No: 0 Name: PRACH
CFN: 7

Message Details:

#### CPHY Transport Channel Release REQ

LLA PHY @ 00:13:44.310

BTS unit: 1:1
Channel No: 0 Name: PRACH
CFN: 8

Message Details:

#### CPHY Transport Channel Release CNF

PHY LLA @ 00:13:44.310

BTS unit: 1:1
Channel No: 0 Name: PRACH
CFN: 8

Message Details:

#### CMAC_Config_CNF

LLA RRC @ 00:13:44.320

Channel ID: PRACH#1
Cell ID: 0

Message Details:

CMAC_Config_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:8

#### CPHY_TrCH_Release_REQ

RRC LLA @ 00:13:44.320

Channel ID: PRACH#1
Cell ID: 0

Message Details:

CPHY_TrCH_Release_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:8

trchConfigType:

nonDch:

#### CPHY_TrCH_Release_CNF

LLA RRC @ 00:13:44.330

Channel ID: PRACH#1
Cell ID: 0

Message Details:

CPHY_TrCH_Release_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:8

#### CPHY_RL_Release_REQ

RRC LLA @ 00:13:44.330

Channel ID: AICH#1
Cell ID: 0

Message Details:

CPHY_RL_Release_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:7

#### CPHY Radio Link Release REQ

LLA PHY @ 00:13:44.330

BTS unit: 1:1
Channel No: 0 Name: AICH
CFN: 10

Message Details:

#### CPHY Radio Link Release CNF

PHY LLA @ 00:13:44.330

BTS unit: 1:1
Channel No: 0 Name: AICH
CFN: 10

Message Details:

#### CPHY_RL_Release_CNF

LLA RRC @ 00:13:44.350

Channel ID: AICH#1
Cell ID: 0

Message Details:

CPHY_RL_Release_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:7

#### CPHY_RL_Release_REQ

RRC LLA @ 00:13:44.350

Channel ID: PRACH#1
Cell ID: 0

Message Details:

CPHY_RL_Release_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:8

#### CPHY Radio Link Release REQ

LLA PHY @ 00:13:44.350

BTS unit: 1:1
Channel No: 0 Name: PRACH
CFN: 12

Message Details:

#### CPHY Radio Link Release CNF

PHY LLA @ 00:13:44.350

BTS unit: 1:1
Channel No: 0 Name: PRACH
CFN: 12

Message Details:

#### CPHY_RL_Release_CNF

LLA RRC @ 00:13:44.360

Channel ID: PRACH#1
Cell ID: 0

Message Details:

CPHY_RL_Release_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:8

#### CRLC_Config_REQ

RRC LLA @ 00:13:44.360

Channel ID: RbPcch
Cell ID: 0

Message Details:

CRLC_Config_REQ:

cellId:0

routingInfo:

rB_Identity:-2

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC TM Channel Release REQ

LLA RLC @ 00:13:44.360

BTS unit: 1:1
Channel No: 0 Name: PCCH
CFN: 13

Message Details:

#### CRLC TM Channel Release CNF

RLC LLA @ 00:13:44.360

BTS unit: 1:1
Channel No: 0 Name: PCCH
CFN: 13

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:13:44.380

Channel ID: RbPcch
Cell ID: 0

Message Details:

CRLC_Config_CNF:

cellId:0

routingInfo:

rB_Identity:-2

#### CMAC_Config_REQ

RRC LLA @ 00:13:44.380

Channel ID: S-CCPCH#1
Cell ID: 0

Message Details:

CMAC_Config_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:5

ratType:fdd

configMessage:

release:

#### CMAC Configuration REQ

LLA MAC @ 00:13:44.380

BTS unit: 1:1
Channel No: 0 Name: S_CCPCH
CFN: 15

Message Details:

Configuration Parameters:

Number Of Transport Channels:0
Active Flag:0

Transport Format Combination Set:

Number Of Transport Format Combinations:0

#### CMAC Configuration CNF

MAC LLA @ 00:13:44.380

BTS unit: 1:1
Channel No: 0 Name: S_CCPCH
CFN: 15

Message Details:

#### CMAC_Config_CNF

LLA RRC @ 00:13:44.390

Channel ID: S-CCPCH#1
Cell ID: 0

Message Details:

CMAC_Config_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:5

#### CPHY_TrCH_Release_REQ

RRC LLA @ 00:13:44.390

Channel ID: S-CCPCH#1
Cell ID: 0

Message Details:

CPHY_TrCH_Release_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:5

trchConfigType:

nonDch:

#### CPHY Transport Channel Release REQ

LLA PHY @ 00:13:44.390

BTS unit: 1:1
Channel No: 0 Name: S_CCPCH
CFN: 16

Message Details:

#### CPHY Transport Channel Release CNF

PHY LLA @ 00:13:44.390

BTS unit: 1:1
Channel No: 0 Name: S_CCPCH
CFN: 16

Message Details:

#### CPHY_TrCH_Release_CNF

LLA RRC @ 00:13:44.410

Channel ID: S-CCPCH#1
Cell ID: 0

Message Details:

CPHY_TrCH_Release_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:5

#### CPHY_RL_Release_REQ

RRC LLA @ 00:13:44.410

Channel ID: PICH#1
Cell ID: 0

Message Details:

CPHY_RL_Release_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:6

#### CPHY Radio Link Release REQ

LLA PHY @ 00:13:44.410

BTS unit: 1:1
Channel No: 0 Name: PICH
CFN: 18

Message Details:

#### CPHY Radio Link Release CNF

PHY LLA @ 00:13:44.410

BTS unit: 1:1
Channel No: 0 Name: PICH
CFN: 18

Message Details:

#### CPHY Radio Link Release REQ

LLA PHY @ 00:13:44.420

BTS unit: 1:1
Channel No: 0 Name: S_CCPCH
CFN: 19

Message Details:

#### CPHY Radio Link Release CNF

PHY LLA @ 00:13:44.420

BTS unit: 1:1
Channel No: 0 Name: S_CCPCH
CFN: 19

Message Details:

#### CPHY_RL_Release_CNF

LLA RRC @ 00:13:44.430

Channel ID: PICH#1
Cell ID: 0

Message Details:

CPHY_RL_Release_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:6

#### CPHY_RL_Release_REQ

RRC LLA @ 00:13:44.430

Channel ID: S-CCPCH#1
Cell ID: 0

Message Details:

CPHY_RL_Release_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:5

#### CPHY_RL_Release_CNF

LLA RRC @ 00:13:44.440

Channel ID: S-CCPCH#1
Cell ID: 0

Message Details:

CPHY_RL_Release_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:5

#### CRLC_Config_REQ

RRC LLA @ 00:13:44.440

Channel ID: RbBcch
Cell ID: 0

Message Details:

CRLC_Config_REQ:

cellId:0

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC TM Channel Release REQ

LLA RLC @ 00:13:44.440

BTS unit: 1:1
Channel No: 0 Name: BCCH
CFN: 21

Message Details:

#### CRLC TM Channel Release CNF

RLC LLA @ 00:13:44.440

BTS unit: 1:1
Channel No: 0 Name: BCCH
CFN: 21

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:13:44.460

Channel ID: RbBcch
Cell ID: 0

Message Details:

CRLC_Config_CNF:

cellId:0

routingInfo:

rB_Identity:-1

#### CMAC_Config_REQ

RRC LLA @ 00:13:44.460

Channel ID: P-CCPCH
Cell ID: 0

Message Details:

CMAC_Config_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:4

ratType:fdd

configMessage:

release:

#### CMAC Configuration REQ

LLA MAC @ 00:13:44.460

BTS unit: 1:1
Channel No: 0 Name: P_CCPCH
CFN: 23

Message Details:

Configuration Parameters:

Number Of Transport Channels:0
Active Flag:0

Transport Format Combination Set:

Number Of Transport Format Combinations:0

#### CMAC Configuration CNF

MAC LLA @ 00:13:44.460

BTS unit: 1:1
Channel No: 0 Name: P_CCPCH
CFN: 23

Message Details:

#### CMAC_Config_CNF

LLA RRC @ 00:13:44.490

Channel ID: P-CCPCH
Cell ID: 0

Message Details:

CMAC_Config_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:4

#### CPHY_TrCH_Release_REQ

RRC LLA @ 00:13:44.490

Channel ID: P-CCPCH
Cell ID: 0

Message Details:

CPHY_TrCH_Release_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:4

trchConfigType:

nonDch:

#### CPHY Transport Channel Release REQ

LLA PHY @ 00:13:44.490

BTS unit: 1:1
Channel No: 0 Name: P_CCPCH
CFN: 26

Message Details:

#### CPHY Transport Channel Release CNF

PHY LLA @ 00:13:44.490

BTS unit: 1:1
Channel No: 0 Name: P_CCPCH
CFN: 26

Message Details:

#### CPHY_TrCH_Release_CNF

LLA RRC @ 00:13:44.500

Channel ID: P-CCPCH
Cell ID: 0

Message Details:

CPHY_TrCH_Release_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:4

#### CPHY_RL_Release_REQ

RRC LLA @ 00:13:44.500

Channel ID: S-SCH
Cell ID: 0

Message Details:

CPHY_RL_Release_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:2

#### CPHY Radio Link Release REQ

LLA PHY @ 00:13:44.500

BTS unit: 1:1
Channel No: 0 Name: S_SCH
CFN: 27

Message Details:

#### CPHY Radio Link Release CNF

PHY LLA @ 00:13:44.500

BTS unit: 1:1
Channel No: 0 Name: S_SCH
CFN: 27

Message Details:

#### CPHY_RL_Release_CNF

LLA RRC @ 00:13:44.520

Channel ID: S-SCH
Cell ID: 0

Message Details:

CPHY_RL_Release_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:2

#### CPHY_RL_Release_REQ

RRC LLA @ 00:13:44.520

Channel ID: P-SCH
Cell ID: 0

Message Details:

CPHY_RL_Release_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:1

#### CPHY Radio Link Release REQ

LLA PHY @ 00:13:44.520

BTS unit: 1:1
Channel No: 0 Name: P_SCH
CFN: 29

Message Details:

#### CPHY Radio Link Release CNF

PHY LLA @ 00:13:44.520

BTS unit: 1:1
Channel No: 0 Name: P_SCH
CFN: 29

Message Details:

#### CPHY Radio Link Release REQ

LLA PHY @ 00:13:44.530

BTS unit: 1:1
Channel No: 0 Name: P_CCPCH
CFN: 30

Message Details:

#### CPHY Radio Link Release CNF

PHY LLA @ 00:13:44.530

BTS unit: 1:1
Channel No: 0 Name: P_CCPCH
CFN: 30

Message Details:

#### CPHY_RL_Release_CNF

LLA RRC @ 00:13:44.540

Channel ID: P-SCH
Cell ID: 0

Message Details:

CPHY_RL_Release_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:1

#### CPHY_RL_Release_REQ

RRC LLA @ 00:13:44.540

Channel ID: P-CCPCH
Cell ID: 0

Message Details:

CPHY_RL_Release_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:4

#### CPHY_RL_Release_CNF

LLA RRC @ 00:13:44.550

Channel ID: P-CCPCH
Cell ID: 0

Message Details:

CPHY_RL_Release_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:4

#### CPHY_RL_Release_REQ

RRC LLA @ 00:13:44.550

Channel ID: P-CPICH
Cell ID: 0

Message Details:

CPHY_RL_Release_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:0

#### CPHY Radio Link Release REQ

LLA PHY @ 00:13:44.550

BTS unit: 1:1
Channel No: 0 Name: P_CPICH
CFN: 32

Message Details:

#### CPHY Radio Link Release CNF

PHY LLA @ 00:13:44.550

BTS unit: 1:1
Channel No: 0 Name: P_CPICH
CFN: 32

Message Details:

#### CPHY_RL_Release_CNF

LLA RRC @ 00:13:44.570

Channel ID: P-CPICH
Cell ID: 0

Message Details:

CPHY_RL_Release_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:0

#### CGEN Stop REQ

RRC PHY @ 00:13:45.610

Message Details:

#### CGEN Stop CNF

PHY RRC @ 00:13:45.610

Message Details: