| NAS_wk34-tc_12_4_1_4c2ps_2004-10-05_16.40.51

#### MMI_CmdReq

RRC |  | LLA | @ 00:00:05.770

| Message Details:
| MMI_CmdReq:
cmd (IA5String): | Please set UE in operation mode A (to support simulataneous CS and PS services)

#### CPHY INI REQ

RRC |  | PHY | @ 00:00:06.030

| Message Details:
RAN Protocol Specification: | 2003-03 R99
| Physical Layer Parameters:
Timing: | Output
Clock: | Output
ISDN Board: | ISDN
| Layer 2 Parameters:
TM bit mode: | enabled

#### CPHY INI CNF

PHY |  | RRC | @ 00:00:06.770

| Message Details:
CAPI Version: | 2.10E1_CIPHER
Release: | MX785201A_2_10E1_A_CT_SEP04_C_CIPHER
| MD8480 pool:
| BTS Group 1:
Software: | V5.10a_Cipher
FPGA: | V5.10
| Hardware Slots:
0: | TIMING GENERATOR
1: | TX BASEBAND
2: | TX BASEBAND
3: | TX BASEBAND
4: | FRAME CODER
5: | FRAME CODER
6: | RX BASEBAND
9: | ISDN V5.10a
10: | RX BASEBAND
12: | FRAME DECODER
13: | VOICE CODEC
14: | TDMA V5.10a
15: | CPU
| Options:
0: | Tx Diversity
1: | Compressed Mode
2: | Integrity & Ciphering
3: | V5.00
4: | Customer1
5: | TS34.121
6: | Router Connection
7: | CSD
| Physical Layer Parameters:
Timing: | Output
Clock: | Output
ISDN Board: | ISDN

#### MMI_CmdCnf

LLA |  | RRC | @ 00:00:08.690

| Message Details:
| MMI_CmdCnf:
result: | true
resultString (IA5String): | Omit

#### MMI_CmdReq

RRC |  | LLA | @ 00:00:08.690

| Message Details:
| MMI_CmdReq:
cmd (IA5String): | Please switch off the UE

#### MMI_CmdCnf

LLA |  | RRC | @ 00:00:09.220

| Message Details:
| MMI_CmdCnf:
result: | true
resultString (IA5String): | Omit

#### CPHY_Ini_REQ

RRC |  | LLA | @ 00:00:09.220

| Message Details:
CPHY_Ini_REQ: | defaultRadioEnvironment

#### CPHY BTS Configuration REQ

LLA |  | PHY | @ 00:00:09.410

| BTS unit: |  | 1:1
| CFN: |  | 182

| Message Details:
| Configuration Parameters:
Power Mode: | Normal Power Mode
RF Connector: | Main
Baseband Adder: | Off
LVDS: | Off
Timing: | 0
Delta Frequency: | 0
Delta Phase: | 0
| Downlink Parameters:
Frequency: | 2140000000
| Uplink Parameters:
Frequency: | 1950000000
| Tx Parameters:
Baseband Connector: | Analogue
Baseband Delay: | Not Used
| CCH Parameters:
Coder: | Tx Coder1 #1
Baseband: | Tx Baseband1
RF: | Tx RF #1
| DCH Parameters:
Coder: | Tx Coder1 #2
Baseband: | Tx Baseband1
RF: | Tx RF #1
| Rx Parameters:
Baseband Connector: | RF
RxMode: | Simultaneous PRACH/UL_DPCH
| CCH Parameters:
Coder: | Rx Decoder1 #1
Baseband: | Rx Baseband1
RF: | Rx RF #1
| DCH Parameters:
Coder: | Rx Decoder1 #2
Baseband: | Rx Baseband1
RF: | Rx RF #1

#### CPHY BTS Configuration CNF

PHY |  | LLA | @ 00:00:09.410

| BTS unit: |  | 1:1
| CFN: |  | 182

| Message Details:

#### CPHY BTS Configuration REQ

LLA |  | PHY | @ 00:00:09.420

| BTS unit: |  | 1:2
| CFN: |  | 183

| Message Details:
| Configuration Parameters:
Power Mode: | Normal Power Mode
RF Connector: | Main
Baseband Adder: | On
LVDS: | Off
Timing: | 0
Delta Frequency: | 0
Delta Phase: | 0
| Downlink Parameters:
Frequency: | 2140000000
| Uplink Parameters:
Frequency: | 1950000000
| Tx Parameters:
Baseband Connector: | Analogue
Baseband Delay: | Not Used
| CCH Parameters:
Coder: | Tx Coder2 #1
Baseband: | Tx Baseband2
RF: | Tx RF #2
| DCH Parameters:
Coder: | Tx Coder1 #2
Baseband: | Tx Baseband2
RF: | Tx RF #2
| Rx Parameters:
Baseband Connector: | RF
RxMode: | Simultaneous PRACH/UL_DPCH
| CCH Parameters:
Coder: | Rx Decoder1 #1
Baseband: | Rx Baseband2
RF: | Rx RF #2
| DCH Parameters:
Coder: | Rx Decoder1 #2
Baseband: | Rx Baseband2
RF: | Rx RF #2

#### CPHY BTS Configuration REQ

LLA |  | PHY | @ 00:00:09.420

| BTS unit: |  | 1:3
| CFN: |  | 183

| Message Details:
| Configuration Parameters:
Power Mode: | Normal Power Mode
RF Connector: | Main
Baseband Adder: | Off
LVDS: | Off
Timing: | 0
Delta Frequency: | 0
Delta Phase: | 0
| Downlink Parameters:
Frequency: | 2140000000
| Uplink Parameters:
Frequency: | 1950000000
| Tx Parameters:
Baseband Connector: | Not Connected
Baseband Delay: | Not Used
| CCH Parameters:
Coder: | Tx Coder2 #2
Baseband: | Tx Baseband3
RF: | Tx RF #2
| DCH Parameters:
Coder: | Tx Coder1 #2
Baseband: | Tx Baseband3
RF: | Tx RF #2
| Rx Parameters:
Baseband Connector: | Not Connected
RxMode: | Single PRACH/UL_DPCH
| CCH Parameters:
Coder: | Not Used
Baseband: | Not Used
RF: | Not Used
| DCH Parameters:
Coder: | Not Used
Baseband: | Not Used
RF: | Not Used

#### CPHY BTS Configuration CNF

PHY |  | LLA | @ 00:00:09.420

| BTS unit: |  | 1:2
| CFN: |  | 183

| Message Details:

#### CPHY BTS Attenuation REQ

LLA |  | PHY | @ 00:00:09.430

| BTS unit: |  | 1:1
| CFN: |  | 184

| Message Details:
| Configuration Parameters:
Tx Attenuation In dB: | 5
Rx Reference Power In dBm: | 0

#### CPHY BTS Configuration CNF

PHY |  | LLA | @ 00:00:09.430

| BTS unit: |  | 1:3
| CFN: |  | 184

| Message Details:

#### CPHY BTS Attenuation CNF

PHY |  | LLA | @ 00:00:09.440

| BTS unit: |  | 1:1
| CFN: |  | 185

| Message Details:

#### CPHY BTS Attenuation REQ

LLA |  | PHY | @ 00:00:09.450

| BTS unit: |  | 1:2
| CFN: |  | 186

| Message Details:
| Configuration Parameters:
Tx Attenuation In dB: | 5
Rx Reference Power In dBm: | 0

#### CPHY BTS Attenuation CNF

PHY |  | LLA | @ 00:00:09.450

| BTS unit: |  | 1:2
| CFN: |  | 186

| Message Details:

#### CPHY_Ini_CNF

LLA |  | RRC | @ 00:00:09.520

| Message Details:
| CPHY_Ini_CNF:
confirmation: |

#### CPHY_Cell_Config_REQ

RRC |  | LLA | @ 00:00:09.520

| Cell ID: |  | 0

| Message Details:
| CPHY_Cell_Config_REQ:
cellId: | 0
tcell: | 0
sfnOffset: | 0
| frequencyInfo:
| modeSpecificInfo:
| fdd: (FrequencyInfoFDD)
uarfcn_UL (UARFCN): | Omit
uarfcn_DL (UARFCN): | 10700
primaryScramblingCode_SS: | 100
| cellTxPowerLevel:
defaultCellTxPowerLvl: |
dLTxAttenuationLevel: | 0

#### CPHY BTS Frequency REQ

LLA |  | PHY | @ 00:00:09.530

| BTS unit: |  | 1:1
| CFN: |  | 194

| Message Details:
| Configuration Parameters:
Down Link Frequency: | 2140000000
Up Link Frequency: | 1950000000

#### CPHY BTS Frequency CNF

PHY |  | LLA | @ 00:00:09.530

| BTS unit: |  | 1:1
| CFN: |  | 194

| Message Details:

#### CPHY_Cell_Config_CNF

LLA |  | RRC | @ 00:00:09.540

| Cell ID: |  | 0

| Message Details:
| CPHY_Cell_Config_CNF:
cellId: | 0

#### CPHY_RL_Setup_REQ

RRC |  | LLA | @ 00:00:09.540

| Channel ID: |  | P-CPICH
| Cell ID: |  | 0

| Message Details:
| CPHY_RL_Setup_REQ:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 0
ratType: | fdd
| setupMessage: (CphyRlSetupReq)
| physicalChannelInfo:
| primaryCPICHInfo:
dl_TxPower_PCPICH: | -60
txdiversityIndicator: | false

#### CPHY Radio Link Setup REQ

LLA |  | PHY | @ 00:00:09.540

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: P_CPICH
| CFN: |  | 195

| Message Details:
| Configuration Parameters:
Channel Offset: | 7680
Scrambling Code: | 1600
Symbol Rate: | 15k
Channelization Code: | 0
Adjust Time: | 0
Power in dBm: | -40
Tx Diversity: | Off
NumOfDpdch: | 0

#### CPHY Radio Link Setup CNF

PHY |  | LLA | @ 00:00:09.540

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: P_CPICH
| CFN: |  | 195

| Message Details:

#### CPHY_RL_Setup_CNF

LLA |  | RRC | @ 00:00:09.550

| Channel ID: |  | P-CPICH
| Cell ID: |  | 0

| Message Details:
| CPHY_RL_Setup_CNF:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 0

#### CPHY_RL_Setup_REQ

RRC |  | LLA | @ 00:00:09.550

| Channel ID: |  | P-SCH
| Cell ID: |  | 0

| Message Details:
| CPHY_RL_Setup_REQ:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 1
ratType: | fdd
| setupMessage: (CphyRlSetupReq)
| physicalChannelInfo:
| primarySCHInfo:
tstdIndicator: | false
dl_TxPower: | -5

#### CPHY Radio Link Setup REQ

LLA |  | PHY | @ 00:00:09.560

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: P_SCH
| CFN: |  | 197

| Message Details:
| Configuration Parameters:
Channel Offset: | 7680
Adjust Time: | 0
Power in dBm: | -45
Tx Diversity: | Off
NumOfDpdch: | 0

#### CPHY Radio Link Setup CNF

PHY |  | LLA | @ 00:00:09.560

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: P_SCH
| CFN: |  | 197

| Message Details:

#### CPHY_RL_Setup_CNF

LLA |  | RRC | @ 00:00:09.570

| Channel ID: |  | P-SCH
| Cell ID: |  | 0

| Message Details:
| CPHY_RL_Setup_CNF:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 1

#### CPHY_RL_Setup_REQ

RRC |  | LLA | @ 00:00:09.570

| Channel ID: |  | S-SCH
| Cell ID: |  | 0

| Message Details:
| CPHY_RL_Setup_REQ:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 2
ratType: | fdd
| setupMessage: (CphyRlSetupReq)
| physicalChannelInfo:
| secondarySCHInfo:
tstdIndicator: | false
dl_TxPower: | -5

#### CPHY Radio Link Setup REQ

LLA |  | PHY | @ 00:00:09.570

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: S_SCH
| CFN: |  | 198

| Message Details:
| Configuration Parameters:
Channel Offset: | 7680
Adjust Time: | 0
Power in dBm: | -45
Tx Diversity: | Off
NumOfDpdch: | 0

#### CPHY Radio Link Setup CNF

PHY |  | LLA | @ 00:00:09.570

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: S_SCH
| CFN: |  | 198

| Message Details:

#### CPHY_RL_Setup_CNF

LLA |  | RRC | @ 00:00:09.580

| Channel ID: |  | S-SCH
| Cell ID: |  | 0

| Message Details:
| CPHY_RL_Setup_CNF:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 2

#### CPHY_RL_Setup_REQ

RRC |  | LLA | @ 00:00:09.580

| Channel ID: |  | P-CCPCH
| Cell ID: |  | 0

| Message Details:
| CPHY_RL_Setup_REQ:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 4
ratType: | fdd
| setupMessage: (CphyRlSetupReq)
| physicalChannelInfo:
| primaryCCPCHInfo:
sttd_Indicator: | false
dl_TxPower: | -2

#### CPHY Radio Link Setup REQ

LLA |  | PHY | @ 00:00:09.590

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: P_CCPCH
| CFN: |  | 200

| Message Details:
| Configuration Parameters:
Channel Offset: | 7680
SFN Offset: | 0
Scrambling Code: | 1600
Symbol Rate: | 15k
Channelization Code: | 1
Adjust Time: | 0
Power in dBm: | -42
Tx Diversity: | Off
NumOfDpdch: | 1

#### CPHY Radio Link Setup CNF

PHY |  | LLA | @ 00:00:09.590

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: P_CCPCH
| CFN: |  | 200

| Message Details:

#### CPHY_RL_Setup_CNF

LLA |  | RRC | @ 00:00:09.600

| Channel ID: |  | P-CCPCH
| Cell ID: |  | 0

| Message Details:
| CPHY_RL_Setup_CNF:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 4

#### CPHY_TrCH_Config_REQ

RRC |  | LLA | @ 00:00:09.600

| Channel ID: |  | P-CCPCH
| Cell ID: |  | 0

| Message Details:
| CPHY_TrCH_Config_REQ:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 4
ratType: | fdd
| trchConfigType:
nonDch: |
| configMessage: (CphyTrchConfigReq)
| activationTime: (SS_ActivationTime)
activateNow: |
| ulconnectedTrCHList: Omit
| ulTFCS: (TFCS) Omit
| dlconnectedTrCHList:
| :
trchid (TransportChannelIdentity): | 11
dl_TransportChannelType (SS_DL_TransportChannelType): | bch
| transportChannelInfo: (CommonOrDedicatedTFS)
| tti:
| tti20: (CommonOrDedicatedTF_InfoList)
| CommonOrDedicatedTF_Info:
tb_Size: | 246
| numberOfTbSizeList:
| NumberOfTransportBlocks:
one: |
| logicalChannelList:
configured: |
| semistaticTF_Information:
| channelCodingType:
convolutional (CodingRate): | half
rateMatchingAttribute: | 1
crc_Size: | crc16
| dlTFCS: (TFCS)
| normalTFCI_Signalling: (ExplicitTFCS_Configuration)
| complete: (TFCS_ReconfAdd)
| ctfcSize:
| ctfc2Bit:
| :
ctfc2: | 0
| powerOffsetInformation:
| gainFactorInformation:
| signalledGainFactors:
| modeSpecificInfo:
| fdd:
gainFactorBetaC (GainFactor): | 11
gainFactorBetaD (GainFactor): | 15
referenceTFC_ID: | 0
powerOffsetPp_m: | Omit

#### CPHY Transport Channel Configuration REQ

LLA |  | PHY | @ 00:00:09.760

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: P_CCPCH
| CFN: |  | 217

| Message Details:
| Configuration Parameters:
DTX Position: | Flexible
Second Interleave: | On
Puncture Limit: | 0
CCTrCH Length: | 270
Number Of Transport Channels: | 1
| Transport Channels:
| Item Number 0:
| Transport Channel Parameters:
| Transport Channel:
Name: | BCH
Identity: | 0
TTI (ms): | 20
EP Type: | 1/2 Rate Convolutional Coding
CRC Size: | 16
RM Attribute: | 1
First Interleave: | On
Number Of Transport Formats: | 2
| Transport Format Set:
| Transport Format 0:
Number Of Transport Blocks: | 0
Transport Block Size In Bits: | 0
| Transport Format 1:
Number Of Transport Blocks: | 1
Transport Block Size In Bits: | 246
RM Maximum Length: | 540
| Transport Format Combination Set:
Number Of Transport Format Combinations: | 2
| Transport Format Combinations 0:
Transport Format: | 0
| Transport Format Combinations 1:
Transport Format: | 1

#### CPHY Transport Channel Configuration CNF

PHY |  | LLA | @ 00:00:09.760

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: P_CCPCH
| CFN: |  | 217

| Message Details:

#### CPHY_TrCH_Config_CNF

LLA |  | RRC | @ 00:00:09.770

| Channel ID: |  | P-CCPCH
| Cell ID: |  | 0

| Message Details:
| CPHY_TrCH_Config_CNF:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 4

#### CMAC_Config_REQ

RRC |  | LLA | @ 00:00:09.770

| Channel ID: |  | P-CCPCH
| Cell ID: |  | 0

| Message Details:
| CMAC_Config_REQ:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 4
ratType: | fdd
| configMessage:
| setup: (CmacConfigReq)
| activationTime: (SS_ActivationTime)
activateNow: |
| uE_Info:
| u_RNTI: Omit
c_RNTI: | Omit
| trCHInfo:
| ulconnectedTrCHList: Omit
| ulTFCS: (TFCS) Omit
| dlconnectedTrCHList:
| :
trchid (TransportChannelIdentity): | 11
| transportChannelInfo: (CommonOrDedicatedTFS)
| tti:
| tti20: (CommonOrDedicatedTF_InfoList)
| CommonOrDedicatedTF_Info:
tb_Size: | 246
| numberOfTbSizeList:
| NumberOfTransportBlocks:
one: |
| logicalChannelList:
configured: |
| semistaticTF_Information:
| channelCodingType:
convolutional (CodingRate): | half
rateMatchingAttribute: | 1
crc_Size: | crc16
| dlTFCS: (TFCS)
| normalTFCI_Signalling: (ExplicitTFCS_Configuration)
| complete: (TFCS_ReconfAdd)
| ctfcSize:
| ctfc2Bit:
| :
ctfc2: | 0
| powerOffsetInformation:
| gainFactorInformation:
| signalledGainFactors:
| modeSpecificInfo:
| fdd:
gainFactorBetaC (GainFactor): | 11
gainFactorBetaD (GainFactor): | 15
referenceTFC_ID: | 0
powerOffsetPp_m: | Omit
| trCH_LogCHMapping: (TrCH_LogCHMappingList1)
| ulconnectedTrCHList: Omit
| dlconnectedTrCHList:
| :
trchid (TransportChannelIdentity): | 11
| trCH_LogCHMappingList:
| TrCH_LogicalChannelMapping:
| logicalChannel_Mapping:
| dl_LogicalChannelMapping: (SS_DL_LogicalChannelMapping)
macHeaderManipulation (MAC_HeaderManipulation): | normalMacHeader
dl_TransportChannelType (SS_DL_TransportChannelType): | bch
logicalChannelIdentity: | 1
logicalChannelType: | bCCH
| rlc_SizeList:
configured: |
mac_LogicalChannelPriority: | 1
rB_Identity: | -1
cn_DomainIdentity: | Omit

#### CMAC Configuration REQ

LLA |  | MAC | @ 00:00:09.780

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: P_CCPCH
| CFN: |  | 219

| Message Details:
| Configuration Parameters:
Number Of Transport Channels: | 1
| Transport Channels:
| Item Number 0:
| Transport Channel Parameters:
| Transport Channel:
Name: | BCH
Identity: | 0
TTI (ms): | 20
EP Type: | 1/2 Rate Convolutional Coding
CRC Size: | 16
RM Attribute: | 1
First Interleave: | On
Number Of Transport Formats: | 2
| Transport Format Set:
| Transport Format 0:
Number Of Transport Blocks: | 0
Transport Block Size In Bits: | 0
| Transport Format 1:
Number Of Transport Blocks: | 1
Transport Block Size In Bits: | 246
Number Of Logical Channels: | 1
| Logical Channels:
| Item Number 0:
| Logical Channel:
Name: | BCCH
Identity: | 0
Priority: | 1
CT Length: | 0
CT Value: | 0
TCTF Length: | 0
TCTF Value: | 0
UE ID Type: | Not used
UE ID: | 0
Active Flag: | 1
| Transport Format Combination Set:
Number Of Transport Format Combinations: | 2
| Transport Format Combinations 0:
Transport Format: | 0
| Transport Format Combinations 1:
Transport Format: | 1

#### CMAC Configuration CNF

MAC |  | LLA | @ 00:00:09.780

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: P_CCPCH
| CFN: |  | 219

| Message Details:

#### CMAC_Config_CNF

LLA |  | RRC | @ 00:00:09.790

| Channel ID: |  | P-CCPCH
| Cell ID: |  | 0

| Message Details:
| CMAC_Config_CNF:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 4

#### CPHY_RL_Setup_REQ

RRC |  | LLA | @ 00:00:09.790

| Channel ID: |  | S-CCPCH#1
| Cell ID: |  | 0

| Message Details:
| CPHY_RL_Setup_REQ:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 5
ratType: | fdd
| setupMessage: (CphyRlSetupReq)
| physicalChannelInfo:
| secondaryCCPCHInfo:
scramblingCode: | 0
| dl_ChannelizationCode: (SF256_AndCodeNumber)
sf64: | 1
sCCPCHSlotFormat: | 8
timingOffset: | 0
positionFixedOrFlexible: | flexible
sttd_Indicator: | false
dl_TxPower: | -2
powerOffsetOfTFCI_PO1: | 6
powerOffsetOfPILOT_PO3: | 6

#### CPHY Radio Link Setup REQ

LLA |  | PHY | @ 00:00:09.790

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: S_CCPCH
| CFN: |  | 220

| Message Details:
| Configuration Parameters:
Channel Offset: | 7680
Scrambling Code: | 1600
Symbol Rate: | 60k
Channelization Code: | 1
Adjust Time: | 0
Power in dBm: | -42
Tx Diversity: | Off
Slot Format: | 8
NumOfDpdch: | 1

#### CPHY Radio Link Setup CNF

PHY |  | LLA | @ 00:00:09.790

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: S_CCPCH
| CFN: |  | 220

| Message Details:

#### CPHY_RL_Setup_CNF

LLA |  | RRC | @ 00:00:09.800

| Channel ID: |  | S-CCPCH#1
| Cell ID: |  | 0

| Message Details:
| CPHY_RL_Setup_CNF:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 5

#### CPHY_TrCH_Config_REQ

RRC |  | LLA | @ 00:00:09.800

| Channel ID: |  | S-CCPCH#1
| Cell ID: |  | 0

| Message Details:
| CPHY_TrCH_Config_REQ:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 5
ratType: | fdd
| trchConfigType:
nonDch: |
| configMessage: (CphyTrchConfigReq)
| activationTime: (SS_ActivationTime)
activateNow: |
| ulconnectedTrCHList: Omit
| ulTFCS: (TFCS) Omit
| dlconnectedTrCHList:
| :
trchid (TransportChannelIdentity): | 12
dl_TransportChannelType (SS_DL_TransportChannelType): | pch
| transportChannelInfo: (CommonOrDedicatedTFS)
| tti:
| tti10: (CommonOrDedicatedTF_InfoList)
| CommonOrDedicatedTF_Info:
tb_Size: | 240
| numberOfTbSizeList:
| NumberOfTransportBlocks:
zero: |
| NumberOfTransportBlocks:
one: |
| logicalChannelList:
allSizes: |
| semistaticTF_Information:
| channelCodingType:
convolutional (CodingRate): | half
rateMatchingAttribute: | 230
crc_Size: | crc16
| :
trchid (TransportChannelIdentity): | 13
dl_TransportChannelType (SS_DL_TransportChannelType): | fach
| transportChannelInfo: (CommonOrDedicatedTFS)
| tti:
| tti10: (CommonOrDedicatedTF_InfoList)
| CommonOrDedicatedTF_Info:
tb_Size: | 168
| numberOfTbSizeList:
| NumberOfTransportBlocks:
zero: |
| NumberOfTransportBlocks:
one: |
| NumberOfTransportBlocks:
small: | 2
| logicalChannelList:
allSizes: |
| semistaticTF_Information:
| channelCodingType:
convolutional (CodingRate): | half
rateMatchingAttribute: | 220
crc_Size: | crc16
| :
trchid (TransportChannelIdentity): | 14
dl_TransportChannelType (SS_DL_TransportChannelType): | fach
| transportChannelInfo: (CommonOrDedicatedTFS)
| tti:
| tti10: (CommonOrDedicatedTF_InfoList)
| CommonOrDedicatedTF_Info:
tb_Size: | 360
| numberOfTbSizeList:
| NumberOfTransportBlocks:
zero: |
| NumberOfTransportBlocks:
one: |
| logicalChannelList:
allSizes: |
| semistaticTF_Information:
| channelCodingType:
turbo: |
rateMatchingAttribute: | 130
crc_Size: | crc16
| dlTFCS: (TFCS)
| normalTFCI_Signalling: (ExplicitTFCS_Configuration)
| complete: (TFCS_ReconfAdd)
| ctfcSize:
| ctfc4Bit:
| :
ctfc4: | 0
| powerOffsetInformation:
| gainFactorInformation:
computedGainFactors (ReferenceTFC_ID): | 0
powerOffsetPp_m: | Omit
| :
ctfc4: | 1
| powerOffsetInformation:
| gainFactorInformation:
computedGainFactors (ReferenceTFC_ID): | 0
powerOffsetPp_m: | Omit
| :
ctfc4: | 2
| powerOffsetInformation:
| gainFactorInformation:
computedGainFactors (ReferenceTFC_ID): | 0
powerOffsetPp_m: | Omit
| :
ctfc4: | 3
| powerOffsetInformation:
| gainFactorInformation:
computedGainFactors (ReferenceTFC_ID): | 0
powerOffsetPp_m: | Omit
| :
ctfc4: | 4
| powerOffsetInformation:
| gainFactorInformation:
computedGainFactors (ReferenceTFC_ID): | 0
powerOffsetPp_m: | Omit
| :
ctfc4: | 5
| powerOffsetInformation:
| gainFactorInformation:
computedGainFactors (ReferenceTFC_ID): | 0
powerOffsetPp_m: | Omit
| :
ctfc4: | 6
| powerOffsetInformation:
| gainFactorInformation:
computedGainFactors (ReferenceTFC_ID): | 0
powerOffsetPp_m: | Omit
| :
ctfc4: | 8
| powerOffsetInformation:
| gainFactorInformation:
| signalledGainFactors:
| modeSpecificInfo:
| fdd:
gainFactorBetaC (GainFactor): | 11
gainFactorBetaD (GainFactor): | 15
referenceTFC_ID: | 0
powerOffsetPp_m: | Omit

#### CPHY Transport Channel Configuration REQ

LLA |  | PHY | @ 00:00:09.810

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: S_CCPCH
| CFN: |  | 222

| Message Details:
| Configuration Parameters:
DTX Position: | Flexible
Second Interleave: | On
Puncture Limit: | 100
CCTrCH Length: | 1080
Number Of Transport Channels: | 3
| Transport Channels:
| Item Number 0:
| Transport Channel Parameters:
| Transport Channel:
Name: | PCH
Identity: | 0
TTI (ms): | 10
EP Type: | 1/2 Rate Convolutional Coding
CRC Size: | 16
RM Attribute: | 230
First Interleave: | On
Number Of Transport Formats: | 2
| Transport Format Set:
| Transport Format 0:
Number Of Transport Blocks: | 0
Transport Block Size In Bits: | 240
| Transport Format 1:
Number Of Transport Blocks: | 1
Transport Block Size In Bits: | 240
RM Maximum Length: | 457
| Item Number 1:
| Transport Channel Parameters:
| Transport Channel:
Name: | FACH
Identity: | 0
TTI (ms): | 10
EP Type: | 1/2 Rate Convolutional Coding
CRC Size: | 16
RM Attribute: | 220
First Interleave: | On
Number Of Transport Formats: | 3
| Transport Format Set:
| Transport Format 0:
Number Of Transport Blocks: | 0
Transport Block Size In Bits: | 168
| Transport Format 1:
Number Of Transport Blocks: | 1
Transport Block Size In Bits: | 168
| Transport Format 2:
Number Of Transport Blocks: | 2
Transport Block Size In Bits: | 168
RM Maximum Length: | 623
| Item Number 2:
| Transport Channel Parameters:
| Transport Channel:
Name: | FACH
Identity: | 1
TTI (ms): | 10
EP Type: | Turbo Coding
CRC Size: | 16
RM Attribute: | 130
First Interleave: | On
Number Of Transport Formats: | 2
| Transport Format Set:
| Transport Format 0:
Number Of Transport Blocks: | 0
Transport Block Size In Bits: | 360
| Transport Format 1:
Number Of Transport Blocks: | 1
Transport Block Size In Bits: | 360
RM Maximum Length: | 558
| Transport Format Combination Set:
Number Of Transport Format Combinations: | 8
| Transport Format Combinations 0:
Transport Format: | 0
Transport Format: | 0
Transport Format: | 0
| Transport Format Combinations 1:
Transport Format: | 1
Transport Format: | 0
Transport Format: | 0
| Transport Format Combinations 2:
Transport Format: | 0
Transport Format: | 1
Transport Format: | 0
| Transport Format Combinations 3:
Transport Format: | 1
Transport Format: | 1
Transport Format: | 0
| Transport Format Combinations 4:
Transport Format: | 0
Transport Format: | 2
Transport Format: | 0
| Transport Format Combinations 5:
Transport Format: | 1
Transport Format: | 2
Transport Format: | 0
| Transport Format Combinations 6:
Transport Format: | 0
Transport Format: | 0
Transport Format: | 1
| Transport Format Combinations 7:
Transport Format: | 0
Transport Format: | 1
Transport Format: | 1

#### CPHY Transport Channel Configuration CNF

PHY |  | LLA | @ 00:00:09.810

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: S_CCPCH
| CFN: |  | 222

| Message Details:

#### CPHY_TrCH_Config_CNF

LLA |  | RRC | @ 00:00:09.820

| Channel ID: |  | S-CCPCH#1
| Cell ID: |  | 0

| Message Details:
| CPHY_TrCH_Config_CNF:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 5

#### CMAC_Config_REQ

RRC |  | LLA | @ 00:00:09.820

| Channel ID: |  | S-CCPCH#1
| Cell ID: |  | 0

| Message Details:
| CMAC_Config_REQ:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 5
ratType: | fdd
| configMessage:
| setup: (CmacConfigReq)
| activationTime: (SS_ActivationTime)
activateNow: |
| uE_Info:
| u_RNTI: Omit
c_RNTI: | Omit
| trCHInfo:
| ulconnectedTrCHList: Omit
| ulTFCS: (TFCS) Omit
| dlconnectedTrCHList:
| :
trchid (TransportChannelIdentity): | 12
| transportChannelInfo: (CommonOrDedicatedTFS)
| tti:
| tti10: (CommonOrDedicatedTF_InfoList)
| CommonOrDedicatedTF_Info:
tb_Size: | 240
| numberOfTbSizeList:
| NumberOfTransportBlocks:
zero: |
| NumberOfTransportBlocks:
one: |
| logicalChannelList:
allSizes: |
| semistaticTF_Information:
| channelCodingType:
convolutional (CodingRate): | half
rateMatchingAttribute: | 230
crc_Size: | crc16
| :
trchid (TransportChannelIdentity): | 13
| transportChannelInfo: (CommonOrDedicatedTFS)
| tti:
| tti10: (CommonOrDedicatedTF_InfoList)
| CommonOrDedicatedTF_Info:
tb_Size: | 168
| numberOfTbSizeList:
| NumberOfTransportBlocks:
zero: |
| NumberOfTransportBlocks:
one: |
| NumberOfTransportBlocks:
small: | 2
| logicalChannelList:
allSizes: |
| semistaticTF_Information:
| channelCodingType:
convolutional (CodingRate): | half
rateMatchingAttribute: | 220
crc_Size: | crc16
| :
trchid (TransportChannelIdentity): | 14
| transportChannelInfo: (CommonOrDedicatedTFS)
| tti:
| tti10: (CommonOrDedicatedTF_InfoList)
| CommonOrDedicatedTF_Info:
tb_Size: | 360
| numberOfTbSizeList:
| NumberOfTransportBlocks:
zero: |
| NumberOfTransportBlocks:
one: |
| logicalChannelList:
allSizes: |
| semistaticTF_Information:
| channelCodingType:
turbo: |
rateMatchingAttribute: | 130
crc_Size: | crc16
| dlTFCS: (TFCS)
| normalTFCI_Signalling: (ExplicitTFCS_Configuration)
| complete: (TFCS_ReconfAdd)
| ctfcSize:
| ctfc4Bit:
| :
ctfc4: | 0
| powerOffsetInformation:
| gainFactorInformation:
computedGainFactors (ReferenceTFC_ID): | 0
powerOffsetPp_m: | Omit
| :
ctfc4: | 1
| powerOffsetInformation:
| gainFactorInformation:
computedGainFactors (ReferenceTFC_ID): | 0
powerOffsetPp_m: | Omit
| :
ctfc4: | 2
| powerOffsetInformation:
| gainFactorInformation:
computedGainFactors (ReferenceTFC_ID): | 0
powerOffsetPp_m: | Omit
| :
ctfc4: | 3
| powerOffsetInformation:
| gainFactorInformation:
computedGainFactors (ReferenceTFC_ID): | 0
powerOffsetPp_m: | Omit
| :
ctfc4: | 4
| powerOffsetInformation:
| gainFactorInformation:
computedGainFactors (ReferenceTFC_ID): | 0
powerOffsetPp_m: | Omit
| :
ctfc4: | 5
| powerOffsetInformation:
| gainFactorInformation:
computedGainFactors (ReferenceTFC_ID): | 0
powerOffsetPp_m: | Omit
| :
ctfc4: | 6
| powerOffsetInformation:
| gainFactorInformation:
computedGainFactors (ReferenceTFC_ID): | 0
powerOffsetPp_m: | Omit
| :
ctfc4: | 8
| powerOffsetInformation:
| gainFactorInformation:
| signalledGainFactors:
| modeSpecificInfo:
| fdd:
gainFactorBetaC (GainFactor): | 11
gainFactorBetaD (GainFactor): | 15
referenceTFC_ID: | 0
powerOffsetPp_m: | Omit
| trCH_LogCHMapping: (TrCH_LogCHMappingList1)
| ulconnectedTrCHList: Omit
| dlconnectedTrCHList:
| :
trchid (TransportChannelIdentity): | 12
| trCH_LogCHMappingList:
| TrCH_LogicalChannelMapping:
| logicalChannel_Mapping:
| dl_LogicalChannelMapping: (SS_DL_LogicalChannelMapping)
macHeaderManipulation (MAC_HeaderManipulation): | normalMacHeader
dl_TransportChannelType (SS_DL_TransportChannelType): | pch
logicalChannelIdentity: | 1
logicalChannelType: | pCCH
| rlc_SizeList:
configured: |
mac_LogicalChannelPriority: | 1
rB_Identity: | -2
cn_DomainIdentity: | Omit
| :
trchid (TransportChannelIdentity): | 13
| trCH_LogCHMappingList:
| TrCH_LogicalChannelMapping:
| logicalChannel_Mapping:
| dl_LogicalChannelMapping: (SS_DL_LogicalChannelMapping)
macHeaderManipulation (MAC_HeaderManipulation): | normalMacHeader
dl_TransportChannelType (SS_DL_TransportChannelType): | fach
logicalChannelIdentity: | 5
logicalChannelType: | cCCH
| rlc_SizeList:
configured: |
mac_LogicalChannelPriority: | 1
rB_Identity: | 0
cn_DomainIdentity: | Omit

#### CMAC_Config_CNF

LLA |  | RRC | @ 00:00:09.830

| Channel ID: |  | S-CCPCH#1
| Cell ID: |  | 0

| Message Details:
| CMAC_Config_CNF:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 5

#### CPHY_RL_Setup_REQ

RRC |  | LLA | @ 00:00:09.830

| Channel ID: |  | PICH#1
| Cell ID: |  | 0

| Message Details:
| CPHY_RL_Setup_REQ:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 6
ratType: | fdd
| setupMessage: (CphyRlSetupReq)
| physicalChannelInfo:
| pICHInfo:
| pichinfo: (PICH_Info)
| fdd:
channelisationCode256: | 2
pi_CountPerFrame: | e18
sttd_Indicator: | false
dl_TxPower (PICH_PowerOffset): | -5
sccpchId_associated: | 5

#### CPHY Radio Link Setup REQ

LLA |  | PHY | @ 00:00:09.840

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: PICH
| CFN: |  | 225

| Message Details:
| Configuration Parameters:
Channel Offset: | 0
Scrambling Code: | 1600
Symbol Rate: | 15k
Channelization Code: | 2
Adjust Time: | 0
Power in dBm: | -45
Tx Diversity: | Off
NumOfDpdch: | 0
Np: | 18

#### CPHY Radio Link Setup CNF

PHY |  | LLA | @ 00:00:09.840

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: PICH
| CFN: |  | 225

| Message Details:

#### CPHY_RL_Setup_CNF

LLA |  | RRC | @ 00:00:09.850

| Channel ID: |  | PICH#1
| Cell ID: |  | 0

| Message Details:
| CPHY_RL_Setup_CNF:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 6

#### CPHY_RL_Setup_REQ

RRC |  | LLA | @ 00:00:09.850

| Channel ID: |  | AICH#1
| Cell ID: |  | 0

| Message Details:
| CPHY_RL_Setup_REQ:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 7
ratType: | fdd
| setupMessage: (CphyRlSetupReq)
| physicalChannelInfo:
| aICHInfo:
| aichinfo: (AICH_Info)
channelisationCode256: | 3
sttd_Indicator: | false
aich_TransmissionTiming: | e0
dl_TxPower (AICH_PowerOffset): | -5

#### CPHY Radio Link Setup REQ

LLA |  | PHY | @ 00:00:09.860

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: AICH
| CFN: |  | 227

| Message Details:
| Configuration Parameters:
Channel Offset: | 7680
Scrambling Code: | 1600
Symbol Rate: | 15k
Channelization Code: | 3
Adjust Time: | 0
Power in dBm: | -45
Tx Diversity: | Off
AICH Transmission Timing: | 3 Access Slots
AICH Polarity: | Positive
NumOfDpdch: | 0

#### CPHY Radio Link Setup CNF

PHY |  | LLA | @ 00:00:09.860

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: AICH
| CFN: |  | 227

| Message Details:

#### CPHY_RL_Setup_CNF

LLA |  | RRC | @ 00:00:09.880

| Channel ID: |  | AICH#1
| Cell ID: |  | 0

| Message Details:
| CPHY_RL_Setup_CNF:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 7

#### CPHY_RL_Setup_REQ

RRC |  | LLA | @ 00:00:09.880

| Channel ID: |  | PRACH#1
| Cell ID: |  | 0

| Message Details:
| CPHY_RL_Setup_REQ:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 8
ratType: | fdd
| setupMessage: (CphyRlSetupReq)
| physicalChannelInfo:
| pRACHInfo:
| fdd_tdd:
| fdd:
preambleSignature (AvailableSignatures): | 0000000011111111
spreadingFactorForDataPart (SF_PRACH): | sfpr64
preambleScramblingCode (PreambleScramblingCodeWordNumber): | 0
puncturingLimit: | pl1
accessSlot (AvailableSubChannelNumbers): | 111111111111

#### CPHY_RL_Setup_CNF

LLA |  | RRC | @ 00:00:09.890

| Channel ID: |  | PRACH#1
| Cell ID: |  | 0

| Message Details:
| CPHY_RL_Setup_CNF:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 8

#### CPHY_TrCH_Config_REQ

RRC |  | LLA | @ 00:00:09.890

| Channel ID: |  | PRACH#1
| Cell ID: |  | 0

| Message Details:
| CPHY_TrCH_Config_REQ:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 8
ratType: | fdd
| trchConfigType:
nonDch: |
| configMessage: (CphyTrchConfigReq)
| activationTime: (SS_ActivationTime)
activateNow: |
| ulconnectedTrCHList:
| :
trchid (TransportChannelIdentity): | 15
ul_TransportChannelType (SS_UL_TransportChannelType): | rach
| transportChannelInfo: (CommonOrDedicatedTFS)
| tti:
| tti20: (CommonOrDedicatedTF_InfoList)
| CommonOrDedicatedTF_Info:
tb_Size: | 168
| numberOfTbSizeList:
| NumberOfTransportBlocks:
one: |
| logicalChannelList:
configured: |
| CommonOrDedicatedTF_Info:
tb_Size: | 360
| numberOfTbSizeList:
| NumberOfTransportBlocks:
one: |
| logicalChannelList:
configured: |
| semistaticTF_Information:
| channelCodingType:
convolutional (CodingRate): | half
rateMatchingAttribute: | 150
crc_Size: | crc16
| ulTFCS: (TFCS)
| normalTFCI_Signalling: (ExplicitTFCS_Configuration)
| complete: (TFCS_ReconfAdd)
| ctfcSize:
| ctfc2Bit:
| :
ctfc2: | 0
| powerOffsetInformation: Omit
| :
ctfc2: | 1
| powerOffsetInformation: Omit
| dlconnectedTrCHList: Omit
| dlTFCS: (TFCS) Omit

#### CPHY Radio Link Setup REQ

LLA |  | PHY | @ 00:00:09.900

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: PRACH
| CFN: |  | 231

| Message Details:
| Configuration Parameters:
Channel Offset: | 10240
Scrambling Code: | 16778816
Symbol Rate: | 60k
Channelization Code: | 128
Adjust Time: | 0
Slot Format: | 2
NumOfDpdch: | 1

#### CPHY Radio Link Setup CNF

PHY |  | LLA | @ 00:00:09.900

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: PRACH
| CFN: |  | 231

| Message Details:

#### CPHY Transport Channel Configuration REQ

LLA |  | PHY | @ 00:00:09.920

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: PRACH
| CFN: |  | 233

| Message Details:
| Configuration Parameters:
DTX Position: | Flexible
Second Interleave: | On
Puncture Limit: | 100
CCTrCH Length: | 600
Number Of Transport Channels: | 1
| Transport Channels:
| Item Number 0:
| Transport Channel Parameters:
| Transport Channel:
Name: | RACH
Identity: | 0
TTI (ms): | 20
EP Type: | 1/2 Rate Convolutional Coding
CRC Size: | 16
RM Attribute: | 150
First Interleave: | On
Number Of Transport Formats: | 2
| Transport Format Set:
| Transport Format 0:
Number Of Transport Blocks: | 1
Transport Block Size In Bits: | 168
| Transport Format 1:
Number Of Transport Blocks: | 1
Transport Block Size In Bits: | 360
RM Maximum Length: | 600
| Transport Format Combination Set:
Number Of Transport Format Combinations: | 2
| Transport Format Combinations 0:
Transport Format: | 0
| Transport Format Combinations 1:
Transport Format: | 1

#### CPHY Transport Channel Configuration CNF

PHY |  | LLA | @ 00:00:09.930

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: PRACH
| CFN: |  | 234

| Message Details:

#### CPHY_TrCH_Config_CNF

LLA |  | RRC | @ 00:00:09.940

| Channel ID: |  | PRACH#1
| Cell ID: |  | 0

| Message Details:
| CPHY_TrCH_Config_CNF:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 8

#### CMAC_Config_REQ

RRC |  | LLA | @ 00:00:09.940

| Channel ID: |  | PRACH#1
| Cell ID: |  | 0

| Message Details:
| CMAC_Config_REQ:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 8
ratType: | fdd
| configMessage:
| setup: (CmacConfigReq)
| activationTime: (SS_ActivationTime)
activateNow: |
| uE_Info:
| u_RNTI: Omit
c_RNTI: | Omit
| trCHInfo:
| ulconnectedTrCHList:
| :
trchid (TransportChannelIdentity): | 15
| transportChannelInfo: (CommonOrDedicatedTFS)
| tti:
| tti20: (CommonOrDedicatedTF_InfoList)
| CommonOrDedicatedTF_Info:
tb_Size: | 168
| numberOfTbSizeList:
| NumberOfTransportBlocks:
one: |
| logicalChannelList:
configured: |
| CommonOrDedicatedTF_Info:
tb_Size: | 360
| numberOfTbSizeList:
| NumberOfTransportBlocks:
one: |
| logicalChannelList:
configured: |
| semistaticTF_Information:
| channelCodingType:
convolutional (CodingRate): | half
rateMatchingAttribute: | 150
crc_Size: | crc16
| ulTFCS: (TFCS)
| normalTFCI_Signalling: (ExplicitTFCS_Configuration)
| complete: (TFCS_ReconfAdd)
| ctfcSize:
| ctfc2Bit:
| :
ctfc2: | 0
| powerOffsetInformation: Omit
| :
ctfc2: | 1
| powerOffsetInformation: Omit
| dlconnectedTrCHList: Omit
| dlTFCS: (TFCS) Omit
| trCH_LogCHMapping: (TrCH_LogCHMappingList1)
| ulconnectedTrCHList:
| :
trchid (TransportChannelIdentity): | 15
| trCH_LogCHMappingList:
| TrCH_LogicalChannelMapping:
| logicalChannel_Mapping:
| ul_LogicalChannelMapping: (SS_UL_LogicalChannelMapping)
macHeaderManipulation (MAC_HeaderManipulation): | normalMacHeader
ul_TransportChannelType (SS_UL_TransportChannelType): | rach
logicalChannelIdentity: | 5
logicalChannelType: | cCCH
rB_Identity: | 0
cn_DomainIdentity: | Omit
| dlconnectedTrCHList: Omit

#### CMAC Configuration REQ

LLA |  | MAC | @ 00:00:09.950

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: PRACH
| CFN: |  | 236

| Message Details:
| Configuration Parameters:
Number Of Transport Channels: | 1
| Transport Channels:
| Item Number 0:
| Transport Channel Parameters:
| Transport Channel:
Name: | RACH
Identity: | 0
TTI (ms): | 20
EP Type: | 1/2 Rate Convolutional Coding
CRC Size: | 16
RM Attribute: | 150
First Interleave: | On
Number Of Transport Formats: | 2
| Transport Format Set:
| Transport Format 0:
Number Of Transport Blocks: | 1
Transport Block Size In Bits: | 168
| Transport Format 1:
Number Of Transport Blocks: | 1
Transport Block Size In Bits: | 360
Number Of Logical Channels: | 1
| Logical Channels:
| Item Number 0:
| Logical Channel:
Name: | CCCH
Identity: | 0
Priority: | 0
CT Length: | 0
CT Value: | 0
TCTF Length: | 2
TCTF Value: | 0
UE ID Type: | Not used
UE ID: | 0
Active Flag: | 1
| Transport Format Combination Set:
Number Of Transport Format Combinations: | 2
| Transport Format Combinations 0:
Transport Format: | 0
| Transport Format Combinations 1:
Transport Format: | 1

#### CMAC Configuration CNF

MAC |  | LLA | @ 00:00:09.950

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: PRACH
| CFN: |  | 236

| Message Details:

#### CMAC_Config_CNF

LLA |  | RRC | @ 00:00:09.960

| Channel ID: |  | PRACH#1
| Cell ID: |  | 0

| Message Details:
| CMAC_Config_CNF:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 8

#### CPHY_RL_Setup_REQ

RRC |  | LLA | @ 00:00:09.960

| Channel ID: |  | DL-DPCH#1
| Cell ID: |  | 0

| Message Details:
| CPHY_RL_Setup_REQ:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 26
ratType: | fdd
| setupMessage: (CphyRlSetupReq)
| physicalChannelInfo:
| dPCHInfo:
| ul_DPCHInfo: (UL_DPCH_Info) Omit
| dl_DPCHInfo:
| dl_CommonInformation:
| dl_DPCH_InfoCommon:
| cfnHandling:
| initialise:
cfntargetsfnframeoffset: | Omit
| modeSpecificInfo:
| fdd:
| dl_DPCH_PowerControlInfo:
| modeSpecificInfo:
| fdd:
dpc_Mode: | singleTPC
powerOffsetPilot_pdpdch: | 0
| dl_rate_matching_restriction: Omit
| spreadingFactorAndPilot: (SF512_AndPilot)
sfd128 (PilotBits128): | pb4
positionFixedOrFlexible: | fixed
tfci_Existence: | false
| modeSpecificInfo:
| fdd:
defaultDPCH_OffsetValue (DefaultDPCH_OffsetValueFDD): | 0
| dpch_CompressedModeInfo: Omit
tx_DiversityMode: | noDiversity
| ssdt_Information: Omit
| dl_DPCH_InfoPerRL:
| fdd:
pCPICH_UsageForChannelEst: | mayBeUsed
dpch_FrameOffset: | 0
| secondaryCPICH_Info: Omit
| dl_ChannelisationCodeList:
| DL_ChannelisationCode:
secondaryScramblingCode: | 1
| sf_AndCodeNumber: (SF512_AndCodeNumber)
sf128: | 0
scramblingCodeChange: | Omit
tpc_CombinationIndex: | 0
ssdt_CellIdentity: | Omit
closedLoopTimingAdjMode: | Omit
powerOffsetOfTFCI_PO1: | 0
powerOffsetOfTPC_PO2: | 0
powerOffsetOfPILOT_PO3: | 0
dl_TxPower: | -5
dl_TxPowerMax (DL_TxPower): | 15
dl_TxPowerMin (DL_TxPower): | -35

#### CPHY Radio Link Setup REQ

LLA |  | PHY | @ 00:00:09.970

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: D_DPCH
| CFN: |  | 238

| Message Details:
| Configuration Parameters:
Channel Offset: | 7680
Scrambling Code: | 1601
Symbol Rate: | 30k
Channelization Code: | 0
Adjust Time: | 0
Power in dBm: | -45
Tx Diversity: | Off
Slot Format: | 8
Number Of DPDCH: | 1
| DPDCH Parameters:
| Item Number 0:
Power in dBm: | -45
Channelization Code: | 0

#### CPHY Radio Link Setup CNF

PHY |  | LLA | @ 00:00:09.970

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: D_DPCH
| CFN: |  | 238

| Message Details:

#### CPHY_RL_Setup_CNF

LLA |  | RRC | @ 00:00:09.990

| Channel ID: |  | DL-DPCH#1
| Cell ID: |  | 0

| Message Details:
| CPHY_RL_Setup_CNF:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 26

#### CPHY_TrCH_Config_REQ

RRC |  | LLA | @ 00:00:09.990

| Channel ID: |  | DL-DPCH#1
| Cell ID: |  | 0

| Message Details:
| CPHY_TrCH_Config_REQ:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 26
ratType: | fdd
| trchConfigType:
dch: | normal
| configMessage: (CphyTrchConfigReq)
| activationTime: (SS_ActivationTime)
activateNow: |
| ulconnectedTrCHList: Omit
| ulTFCS: (TFCS) Omit
| dlconnectedTrCHList:
| :
trchid (TransportChannelIdentity): | 10
dl_TransportChannelType (SS_DL_TransportChannelType): | dch
| transportChannelInfo: (CommonOrDedicatedTFS)
| tti:
| tti10: (CommonOrDedicatedTF_InfoList)
| CommonOrDedicatedTF_Info:
tb_Size: | 148
| numberOfTbSizeList:
| NumberOfTransportBlocks:
zero: |
| NumberOfTransportBlocks:
one: |
| logicalChannelList:
allSizes: |
| semistaticTF_Information:
| channelCodingType:
convolutional (CodingRate): | third
rateMatchingAttribute: | 192
crc_Size: | crc16
| dlTFCS: (TFCS)
| normalTFCI_Signalling: (ExplicitTFCS_Configuration)
| complete: (TFCS_ReconfAdd)
| ctfcSize:
| ctfc2Bit:
| :
ctfc2: | 0
| powerOffsetInformation:
| gainFactorInformation:
computedGainFactors (ReferenceTFC_ID): | 0
powerOffsetPp_m: | Omit
| :
ctfc2: | 1
| powerOffsetInformation:
| gainFactorInformation:
| signalledGainFactors:
| modeSpecificInfo:
| fdd:
gainFactorBetaC (GainFactor): | 11
gainFactorBetaD (GainFactor): | 15
referenceTFC_ID: | 0
powerOffsetPp_m: | Omit

#### CPHY_TrCH_Config_CNF

LLA |  | RRC | @ 00:00:10.000

| Channel ID: |  | DL-DPCH#1
| Cell ID: |  | 0

| Message Details:
| CPHY_TrCH_Config_CNF:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 26

#### CMAC_Config_REQ

RRC |  | LLA | @ 00:00:10.000

| Channel ID: |  | DL-DPCH#1
| Cell ID: |  | -1

| Message Details:
| CMAC_Config_REQ:
cellId: | -1
| routingInfo:
physicalChannelIdentity: | 26
ratType: | fdd
| configMessage:
| setup: (CmacConfigReq)
| activationTime: (SS_ActivationTime)
activateNow: |
| uE_Info:
| u_RNTI: Omit
c_RNTI: | Omit
| trCHInfo:
| ulconnectedTrCHList: Omit
| ulTFCS: (TFCS) Omit
| dlconnectedTrCHList:
| :
trchid (TransportChannelIdentity): | 10
| transportChannelInfo: (CommonOrDedicatedTFS)
| tti:
| tti10: (CommonOrDedicatedTF_InfoList)
| CommonOrDedicatedTF_Info:
tb_Size: | 148
| numberOfTbSizeList:
| NumberOfTransportBlocks:
zero: |
| NumberOfTransportBlocks:
one: |
| logicalChannelList:
allSizes: |
| semistaticTF_Information:
| channelCodingType:
convolutional (CodingRate): | third
rateMatchingAttribute: | 192
crc_Size: | crc16
| dlTFCS: (TFCS)
| normalTFCI_Signalling: (ExplicitTFCS_Configuration)
| complete: (TFCS_ReconfAdd)
| ctfcSize:
| ctfc2Bit:
| :
ctfc2: | 0
| powerOffsetInformation:
| gainFactorInformation:
computedGainFactors (ReferenceTFC_ID): | 0
powerOffsetPp_m: | Omit
| :
ctfc2: | 1
| powerOffsetInformation:
| gainFactorInformation:
| signalledGainFactors:
| modeSpecificInfo:
| fdd:
gainFactorBetaC (GainFactor): | 11
gainFactorBetaD (GainFactor): | 15
referenceTFC_ID: | 0
powerOffsetPp_m: | Omit
| trCH_LogCHMapping: (TrCH_LogCHMappingList1)
| ulconnectedTrCHList: Omit
| dlconnectedTrCHList:
| :
trchid (TransportChannelIdentity): | 10
| trCH_LogCHMappingList:
| TrCH_LogicalChannelMapping:
| logicalChannel_Mapping:
| dl_LogicalChannelMapping: (SS_DL_LogicalChannelMapping)
macHeaderManipulation (MAC_HeaderManipulation): | normalMacHeader
dl_TransportChannelType (SS_DL_TransportChannelType): | dch
logicalChannelIdentity: | 1
logicalChannelType: | dCCH
| rlc_SizeList:
configured: |
mac_LogicalChannelPriority: | 1
rB_Identity: | 1
cn_DomainIdentity: | Omit
| TrCH_LogicalChannelMapping:
| logicalChannel_Mapping:
| dl_LogicalChannelMapping: (SS_DL_LogicalChannelMapping)
macHeaderManipulation (MAC_HeaderManipulation): | normalMacHeader
dl_TransportChannelType (SS_DL_TransportChannelType): | dch
logicalChannelIdentity: | 2
logicalChannelType: | dCCH
| rlc_SizeList:
configured: |
mac_LogicalChannelPriority: | 2
rB_Identity: | 2
cn_DomainIdentity: | Omit
| TrCH_LogicalChannelMapping:
| logicalChannel_Mapping:
| dl_LogicalChannelMapping: (SS_DL_LogicalChannelMapping)
macHeaderManipulation (MAC_HeaderManipulation): | normalMacHeader
dl_TransportChannelType (SS_DL_TransportChannelType): | dch
logicalChannelIdentity: | 3
logicalChannelType: | dCCH
| rlc_SizeList:
configured: |
mac_LogicalChannelPriority: | 3
rB_Identity: | 3
cn_DomainIdentity: | Omit
| TrCH_LogicalChannelMapping:
| logicalChannel_Mapping:
| dl_LogicalChannelMapping: (SS_DL_LogicalChannelMapping)
macHeaderManipulation (MAC_HeaderManipulation): | normalMacHeader
dl_TransportChannelType (SS_DL_TransportChannelType): | dch
logicalChannelIdentity: | 4
logicalChannelType: | dCCH
| rlc_SizeList:
configured: |
mac_LogicalChannelPriority: | 4
rB_Identity: | 4
cn_DomainIdentity: | Omit

#### CPHY Transport Channel Configuration REQ

LLA |  | PHY | @ 00:00:10.000

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: D_DPCH
| CFN: |  | 241

| Message Details:
| Configuration Parameters:
DTX Position: | Fixed
Second Interleave: | On
Puncture Limit: | 0
CCTrCH Length: | 510
Number Of Transport Channels: | 1
| Transport Channels:
| Item Number 0:
| Transport Channel Parameters:
| Transport Channel:
Name: | D_DCH
Identity: | 0
TTI (ms): | 10
EP Type: | 1/3 Rate Convolutional Coding
CRC Size: | 16
RM Attribute: | 192
First Interleave: | On
Number Of Transport Formats: | 2
| Transport Format Set:
| Transport Format 0:
Number Of Transport Blocks: | 0
Transport Block Size In Bits: | 148
| Transport Format 1:
Number Of Transport Blocks: | 1
Transport Block Size In Bits: | 148
RM Maximum Length: | 510
| Transport Format Combination Set:
Number Of Transport Format Combinations: | 2
| Transport Format Combinations 0:
Transport Format: | 0
| Transport Format Combinations 1:
Transport Format: | 1

#### CPHY Transport Channel Configuration CNF

PHY |  | LLA | @ 00:00:10.000

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: D_DPCH
| CFN: |  | 241

| Message Details:

#### CMAC Configuration REQ

LLA |  | MAC | @ 00:00:10.020

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: D_DPCH
| CFN: |  | 243

| Message Details:
| Configuration Parameters:
Number Of Transport Channels: | 1
| Transport Channels:
| Item Number 0:
| Transport Channel Parameters:
| Transport Channel:
Name: | D_DCH
Identity: | 0
TTI (ms): | 10
EP Type: | 1/3 Rate Convolutional Coding
CRC Size: | 16
RM Attribute: | 192
First Interleave: | On
Number Of Transport Formats: | 2
| Transport Format Set:
| Transport Format 0:
Number Of Transport Blocks: | 0
Transport Block Size In Bits: | 148
| Transport Format 1:
Number Of Transport Blocks: | 1
Transport Block Size In Bits: | 148
Number Of Logical Channels: | 4
| Logical Channels:
| Item Number 0:
| Logical Channel:
Name: | DCCH
Identity: | 1
Priority: | 1
CT Length: | 4
CT Value: | 0
TCTF Length: | 0
TCTF Value: | 0
UE ID Type: | Not used
UE ID: | 0
| Item Number 1:
| Logical Channel:
Name: | DCCH
Identity: | 2
Priority: | 2
CT Length: | 4
CT Value: | 1
TCTF Length: | 0
TCTF Value: | 0
UE ID Type: | Not used
UE ID: | 0
| Item Number 2:
| Logical Channel:
Name: | DCCH
Identity: | 3
Priority: | 3
CT Length: | 4
CT Value: | 2
TCTF Length: | 0
TCTF Value: | 0
UE ID Type: | Not used
UE ID: | 0
| Item Number 3:
| Logical Channel:
Name: | DCCH
Identity: | 4
Priority: | 4
CT Length: | 4
CT Value: | 3
TCTF Length: | 0
TCTF Value: | 0
UE ID Type: | Not used
UE ID: | 0
Active Flag: | 1
| Transport Format Combination Set:
Number Of Transport Format Combinations: | 2
| Transport Format Combinations 0:
Transport Format: | 0
| Transport Format Combinations 1:
Transport Format: | 1

#### CMAC Configuration CNF

MAC |  | LLA | @ 00:00:10.020

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: D_DPCH
| CFN: |  | 243

| Message Details:

#### CMAC_Config_CNF

LLA |  | RRC | @ 00:00:10.040

| Channel ID: |  | DL-DPCH#1
| Cell ID: |  | -1

| Message Details:
| CMAC_Config_CNF:
cellId: | -1
| routingInfo:
physicalChannelIdentity: | 26

#### CPHY_RL_Setup_REQ

RRC |  | LLA | @ 00:00:10.040

| Channel ID: |  | UL-DPCH#1
| Cell ID: |  | 0

| Message Details:
| CPHY_RL_Setup_REQ:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 20
ratType: | fdd
| setupMessage: (CphyRlSetupReq)
| physicalChannelInfo:
| dPCHInfo:
| ul_DPCHInfo: (UL_DPCH_Info)
| ul_DPCH_PowerControlInfo:
| fdd:
dpcch_PowerOffset: | -40
pc_Preamble: | 1
sRB_delay: | 7
| powerControlAlgorithm:
algorithm1 (TPC_StepSizeFDD): | 0
| modeSpecificInfo:
| fdd:
scramblingCodeType: | longSC
scramblingCode (UL_ScramblingCode): | 0
numberOfDPDCH: | Omit
spreadingFactor: | sf64
tfci_Existence: | true
numberOfFBI_Bits: | Omit
puncturingLimit: | pl1
| dl_DPCHInfo: Omit

#### CPHY_RL_Setup_CNF

LLA |  | RRC | @ 00:00:10.050

| Channel ID: |  | UL-DPCH#1
| Cell ID: |  | 0

| Message Details:
| CPHY_RL_Setup_CNF:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 20

#### CPHY_TrCH_Config_REQ

RRC |  | LLA | @ 00:00:10.050

| Channel ID: |  | UL-DPCH#1
| Cell ID: |  | 0

| Message Details:
| CPHY_TrCH_Config_REQ:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 20
ratType: | fdd
| trchConfigType:
dch: | normal
| configMessage: (CphyTrchConfigReq)
| activationTime: (SS_ActivationTime)
activateNow: |
| ulconnectedTrCHList:
| :
trchid (TransportChannelIdentity): | 5
ul_TransportChannelType (SS_UL_TransportChannelType): | dch
| transportChannelInfo: (CommonOrDedicatedTFS)
| tti:
| tti10: (CommonOrDedicatedTF_InfoList)
| CommonOrDedicatedTF_Info:
tb_Size: | 148
| numberOfTbSizeList:
| NumberOfTransportBlocks:
zero: |
| NumberOfTransportBlocks:
one: |
| logicalChannelList:
allSizes: |
| semistaticTF_Information:
| channelCodingType:
convolutional (CodingRate): | third
rateMatchingAttribute: | 192
crc_Size: | crc16
| ulTFCS: (TFCS)
| normalTFCI_Signalling: (ExplicitTFCS_Configuration)
| complete: (TFCS_ReconfAdd)
| ctfcSize:
| ctfc2Bit:
| :
ctfc2: | 0
| powerOffsetInformation: Omit
| :
ctfc2: | 1
| powerOffsetInformation: Omit
| dlconnectedTrCHList: Omit
| dlTFCS: (TFCS) Omit

#### CPHY Radio Link Setup REQ

LLA |  | PHY | @ 00:00:10.060

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: U_DPCH
| CFN: |  | 247

| Message Details:
| Configuration Parameters:
Channel Offset: | 8704
Scrambling Code: | 16777216
Symbol Rate: | 60k
Channelization Code: | 0
Adjust Time: | 0
Slot Format: | 0
Number Of DPDCH: | 1
| DPDCH Parameters:
| Item Number 0:
Channelization Code: | 16

#### CPHY Radio Link Setup CNF

PHY |  | LLA | @ 00:00:10.060

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: U_DPCH
| CFN: |  | 247

| Message Details:

#### CPHY Transport Channel Configuration REQ

LLA |  | PHY | @ 00:00:10.080

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: U_DPCH
| CFN: |  | 249

| Message Details:
| Configuration Parameters:
DTX Position: | Flexible
Second Interleave: | On
Puncture Limit: | 100
CCTrCH Length: | 600
Number Of Transport Channels: | 1
| Transport Channels:
| Item Number 0:
| Transport Channel Parameters:
| Transport Channel:
Name: | U_DCH
Identity: | 0
TTI (ms): | 10
EP Type: | 1/3 Rate Convolutional Coding
CRC Size: | 16
RM Attribute: | 192
First Interleave: | On
Number Of Transport Formats: | 2
| Transport Format Set:
| Transport Format 0:
Number Of Transport Blocks: | 0
Transport Block Size In Bits: | 148
| Transport Format 1:
Number Of Transport Blocks: | 1
Transport Block Size In Bits: | 148
RM Maximum Length: | 600
| Transport Format Combination Set:
Number Of Transport Format Combinations: | 2
| Transport Format Combinations 0:
Transport Format: | 0
| Transport Format Combinations 1:
Transport Format: | 1

#### CPHY Transport Channel Configuration CNF

PHY |  | LLA | @ 00:00:10.090

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: U_DPCH
| CFN: |  | 250

| Message Details:

#### CPHY_TrCH_Config_CNF

LLA |  | RRC | @ 00:00:10.100

| Channel ID: |  | UL-DPCH#1
| Cell ID: |  | 0

| Message Details:
| CPHY_TrCH_Config_CNF:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 20

#### CMAC_Config_REQ

RRC |  | LLA | @ 00:00:10.100

| Channel ID: |  | UL-DPCH#1
| Cell ID: |  | -1

| Message Details:
| CMAC_Config_REQ:
cellId: | -1
| routingInfo:
physicalChannelIdentity: | 20
ratType: | fdd
| configMessage:
| setup: (CmacConfigReq)
| activationTime: (SS_ActivationTime)
activateNow: |
| uE_Info:
| u_RNTI: Omit
c_RNTI: | Omit
| trCHInfo:
| ulconnectedTrCHList:
| :
trchid (TransportChannelIdentity): | 5
| transportChannelInfo: (CommonOrDedicatedTFS)
| tti:
| tti10: (CommonOrDedicatedTF_InfoList)
| CommonOrDedicatedTF_Info:
tb_Size: | 148
| numberOfTbSizeList:
| NumberOfTransportBlocks:
zero: |
| NumberOfTransportBlocks:
one: |
| logicalChannelList:
allSizes: |
| semistaticTF_Information:
| channelCodingType:
convolutional (CodingRate): | third
rateMatchingAttribute: | 192
crc_Size: | crc16
| ulTFCS: (TFCS)
| normalTFCI_Signalling: (ExplicitTFCS_Configuration)
| complete: (TFCS_ReconfAdd)
| ctfcSize:
| ctfc2Bit:
| :
ctfc2: | 0
| powerOffsetInformation: Omit
| :
ctfc2: | 1
| powerOffsetInformation: Omit
| dlconnectedTrCHList: Omit
| dlTFCS: (TFCS) Omit
| trCH_LogCHMapping: (TrCH_LogCHMappingList1)
| ulconnectedTrCHList:
| :
trchid (TransportChannelIdentity): | 5
| trCH_LogCHMappingList:
| TrCH_LogicalChannelMapping:
| logicalChannel_Mapping:
| ul_LogicalChannelMapping: (SS_UL_LogicalChannelMapping)
macHeaderManipulation (MAC_HeaderManipulation): | normalMacHeader
ul_TransportChannelType (SS_UL_TransportChannelType): | dch
logicalChannelIdentity: | 1
logicalChannelType: | dCCH
rB_Identity: | 1
cn_DomainIdentity: | Omit
| TrCH_LogicalChannelMapping:
| logicalChannel_Mapping:
| ul_LogicalChannelMapping: (SS_UL_LogicalChannelMapping)
macHeaderManipulation (MAC_HeaderManipulation): | normalMacHeader
ul_TransportChannelType (SS_UL_TransportChannelType): | dch
logicalChannelIdentity: | 2
logicalChannelType: | dCCH
rB_Identity: | 2
cn_DomainIdentity: | Omit
| TrCH_LogicalChannelMapping:
| logicalChannel_Mapping:
| ul_LogicalChannelMapping: (SS_UL_LogicalChannelMapping)
macHeaderManipulation (MAC_HeaderManipulation): | normalMacHeader
ul_TransportChannelType (SS_UL_TransportChannelType): | dch
logicalChannelIdentity: | 3
logicalChannelType: | dCCH
rB_Identity: | 3
cn_DomainIdentity: | Omit
| TrCH_LogicalChannelMapping:
| logicalChannel_Mapping:
| ul_LogicalChannelMapping: (SS_UL_LogicalChannelMapping)
macHeaderManipulation (MAC_HeaderManipulation): | normalMacHeader
ul_TransportChannelType (SS_UL_TransportChannelType): | dch
logicalChannelIdentity: | 4
logicalChannelType: | dCCH
rB_Identity: | 4
cn_DomainIdentity: | Omit
| dlconnectedTrCHList: Omit

#### CMAC_Config_CNF

LLA |  | RRC | @ 00:00:10.110

| Channel ID: |  | UL-DPCH#1
| Cell ID: |  | -1

| Message Details:
| CMAC_Config_CNF:
cellId: | -1
| routingInfo:
physicalChannelIdentity: | 20

#### CRLC_Config_REQ

RRC |  | LLA | @ 00:00:10.110

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CRLC_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CrlcConfigReq)
| setup: (RBInfo)
| sS_rlc_Info:
| sS_ul_RLC_Mode: (DL_RLC_Mode) Omit
| sS_dl_RLC_Mode:
dl_PayloadSize (PayloadSize): | 246
| dl_RLCModeInfo: (UL_RLC_Mode)
| ul_TM_RLC_Mode:
| transmissionRLC_Discard: Omit
segmentationIndication: | false
| rB_LogCH_Mapping:
uLlogicalChannelIdentity (LogicalChannelIdentity): | Omit
dLlogicalChannelIdentity (LogicalChannelIdentity): | 1
logicalChannelType: | Omit
cn_DomainIdentity: | Omit

#### CMAC Configuration REQ

LLA |  | MAC | @ 00:00:10.110

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: U_DPCH
| CFN: |  | 252

| Message Details:
| Configuration Parameters:
Number Of Transport Channels: | 1
| Transport Channels:
| Item Number 0:
| Transport Channel Parameters:
| Transport Channel:
Name: | U_DCH
Identity: | 0
TTI (ms): | 10
EP Type: | 1/3 Rate Convolutional Coding
CRC Size: | 16
RM Attribute: | 192
First Interleave: | On
Number Of Transport Formats: | 2
| Transport Format Set:
| Transport Format 0:
Number Of Transport Blocks: | 0
Transport Block Size In Bits: | 148
| Transport Format 1:
Number Of Transport Blocks: | 1
Transport Block Size In Bits: | 148
Number Of Logical Channels: | 4
| Logical Channels:
| Item Number 0:
| Logical Channel:
Name: | DCCH
Identity: | 1
Priority: | 0
CT Length: | 4
CT Value: | 0
TCTF Length: | 0
TCTF Value: | 0
UE ID Type: | Not used
UE ID: | 0
| Item Number 1:
| Logical Channel:
Name: | DCCH
Identity: | 2
Priority: | 0
CT Length: | 4
CT Value: | 1
TCTF Length: | 0
TCTF Value: | 0
UE ID Type: | Not used
UE ID: | 0
| Item Number 2:
| Logical Channel:
Name: | DCCH
Identity: | 3
Priority: | 0
CT Length: | 4
CT Value: | 2
TCTF Length: | 0
TCTF Value: | 0
UE ID Type: | Not used
UE ID: | 0
| Item Number 3:
| Logical Channel:
Name: | DCCH
Identity: | 4
Priority: | 0
CT Length: | 4
CT Value: | 3
TCTF Length: | 0
TCTF Value: | 0
UE ID Type: | Not used
UE ID: | 0
Active Flag: | 1
| Transport Format Combination Set:
Number Of Transport Format Combinations: | 2
| Transport Format Combinations 0:
Transport Format: | 0
| Transport Format Combinations 1:
Transport Format: | 1

#### CMAC Configuration CNF

MAC |  | LLA | @ 00:00:10.110

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: U_DPCH
| CFN: |  | 252

| Message Details:

#### CRLC_Config_CNF

LLA |  | RRC | @ 00:00:10.130

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CRLC_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### CRLC_Config_REQ

RRC |  | LLA | @ 00:00:10.130

| Channel ID: |  | RbPcch
| Cell ID: |  | 0

| Message Details:
| CRLC_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -2
ratType: | fdd
| configMessage: (CrlcConfigReq)
| setup: (RBInfo)
| sS_rlc_Info:
| sS_ul_RLC_Mode: (DL_RLC_Mode) Omit
| sS_dl_RLC_Mode:
dl_PayloadSize (PayloadSize): | 240
| dl_RLCModeInfo: (UL_RLC_Mode)
| ul_TM_RLC_Mode:
| transmissionRLC_Discard: Omit
segmentationIndication: | false
| rB_LogCH_Mapping:
uLlogicalChannelIdentity (LogicalChannelIdentity): | Omit
dLlogicalChannelIdentity (LogicalChannelIdentity): | 1
logicalChannelType: | Omit
cn_DomainIdentity: | Omit

#### CRLC_Config_CNF

LLA |  | RRC | @ 00:00:10.140

| Channel ID: |  | RbPcch
| Cell ID: |  | 0

| Message Details:
| CRLC_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -2

#### CRLC_Config_REQ

RRC |  | LLA | @ 00:00:10.140

| Channel ID: |  | Rb0
| Cell ID: |  | 0

| Message Details:
| CRLC_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | 0
ratType: | fdd
| configMessage: (CrlcConfigReq)
| setup: (RBInfo)
| sS_rlc_Info:
| sS_ul_RLC_Mode: (DL_RLC_Mode) Omit
| sS_dl_RLC_Mode:
dl_PayloadSize (PayloadSize): | 152
| dl_RLCModeInfo: (UL_RLC_Mode)
| ul_UM_RLC_Mode:
| transmissionRLC_Discard:
timerBasedNoExplicit (NoExplicitDiscard): | dt100
| rB_LogCH_Mapping:
uLlogicalChannelIdentity (LogicalChannelIdentity): | Omit
dLlogicalChannelIdentity (LogicalChannelIdentity): | 5
logicalChannelType: | Omit
cn_DomainIdentity: | Omit

#### CRLC_Config_CNF

LLA |  | RRC | @ 00:00:10.160

| Channel ID: |  | Rb0
| Cell ID: |  | 0

| Message Details:
| CRLC_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | 0

#### CRLC_Config_REQ

RRC |  | LLA | @ 00:00:10.160

| Channel ID: |  | Rb0
| Cell ID: |  | 0

| Message Details:
| CRLC_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | 0
ratType: | fdd
| configMessage: (CrlcConfigReq)
| setup: (RBInfo)
| sS_rlc_Info:
| sS_ul_RLC_Mode: (DL_RLC_Mode)
| dl_TM_RLC_Mode:
segmentationIndication: | false
| sS_dl_RLC_Mode:
dl_PayloadSize (PayloadSize): | 166
| dl_RLCModeInfo: (UL_RLC_Mode)
| ul_TM_RLC_Mode:
| transmissionRLC_Discard: Omit
segmentationIndication: | false
| rB_LogCH_Mapping:
uLlogicalChannelIdentity (LogicalChannelIdentity): | 5
dLlogicalChannelIdentity (LogicalChannelIdentity): | Omit
logicalChannelType: | Omit
cn_DomainIdentity: | Omit

#### CRLC_Config_CNF

LLA |  | RRC | @ 00:00:10.180

| Channel ID: |  | Rb0
| Cell ID: |  | 0

| Message Details:
| CRLC_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | 0

#### CRLC_Config_REQ

RRC |  | LLA | @ 00:00:10.180

| Channel ID: |  | Rb1
| Cell ID: |  | -1

| Message Details:
| CRLC_Config_REQ:
cellId: | -1
| routingInfo:
rB_Identity: | 1
ratType: | fdd
| configMessage: (CrlcConfigReq)
| setup: (RBInfo)
| sS_rlc_Info:
| sS_ul_RLC_Mode: (DL_RLC_Mode)
dl_UM_RLC_Mode: |
| sS_dl_RLC_Mode:
dl_PayloadSize (PayloadSize): | 136
| dl_RLCModeInfo: (UL_RLC_Mode)
| ul_UM_RLC_Mode:
| transmissionRLC_Discard:
timerBasedNoExplicit (NoExplicitDiscard): | dt100
| rB_LogCH_Mapping:
uLlogicalChannelIdentity (LogicalChannelIdentity): | 1
dLlogicalChannelIdentity (LogicalChannelIdentity): | 1
logicalChannelType: | Omit
cn_DomainIdentity: | Omit

#### CRLC_Config_CNF

LLA |  | RRC | @ 00:00:10.190

| Channel ID: |  | Rb1
| Cell ID: |  | -1

| Message Details:
| CRLC_Config_CNF:
cellId: | -1
| routingInfo:
rB_Identity: | 1

#### CRLC_Config_REQ

RRC |  | LLA | @ 00:00:10.190

| Channel ID: |  | Rb2
| Cell ID: |  | -1

| Message Details:
| CRLC_Config_REQ:
cellId: | -1
| routingInfo:
rB_Identity: | 2
ratType: | fdd
| configMessage: (CrlcConfigReq)
| setup: (RBInfo)
| sS_rlc_Info:
| sS_ul_RLC_Mode: (DL_RLC_Mode)
| dl_AM_RLC_Mode:
inSequenceDelivery: | true
receivingWindowSize: | rw32
| dl_RLC_StatusInfo:
timerStatusProhibit: | tsp200
timerEPC: | Omit
missingPDU_Indicator: | true
timerStatusPeriodic: | Omit
| sS_dl_RLC_Mode:
dl_PayloadSize (PayloadSize): | 128
| dl_RLCModeInfo: (UL_RLC_Mode)
| ul_AM_RLC_Mode:
| transmissionRLC_Discard:
noDiscard (MaxDAT): | dat15
transmissionWindowSize: | tw32
timerRST: | tr500
max_RST (MaxRST): | rst1
| pollingInfo:
timerPollProhibit: | tpp200
timerPoll: | tp200
poll_PDU: | Omit
poll_SDU: | sdu1
lastTransmissionPDU_Poll: | true
lastRetransmissionPDU_Poll: | true
pollWindow: | pw99
timerPollPeriodic: | Omit
| rB_LogCH_Mapping:
uLlogicalChannelIdentity (LogicalChannelIdentity): | 2
dLlogicalChannelIdentity (LogicalChannelIdentity): | 2
logicalChannelType: | Omit
cn_DomainIdentity: | Omit

#### CRLC_Config_CNF

LLA |  | RRC | @ 00:00:10.210

| Channel ID: |  | Rb2
| Cell ID: |  | -1

| Message Details:
| CRLC_Config_CNF:
cellId: | -1
| routingInfo:
rB_Identity: | 2

#### CRLC_Config_REQ

RRC |  | LLA | @ 00:00:10.210

| Channel ID: |  | Rb3
| Cell ID: |  | -1

| Message Details:
| CRLC_Config_REQ:
cellId: | -1
| routingInfo:
rB_Identity: | 3
ratType: | fdd
| configMessage: (CrlcConfigReq)
| setup: (RBInfo)
| sS_rlc_Info:
| sS_ul_RLC_Mode: (DL_RLC_Mode)
| dl_AM_RLC_Mode:
inSequenceDelivery: | true
receivingWindowSize: | rw32
| dl_RLC_StatusInfo:
timerStatusProhibit: | tsp200
timerEPC: | Omit
missingPDU_Indicator: | true
timerStatusPeriodic: | Omit
| sS_dl_RLC_Mode:
dl_PayloadSize (PayloadSize): | 128
| dl_RLCModeInfo: (UL_RLC_Mode)
| ul_AM_RLC_Mode:
| transmissionRLC_Discard:
noDiscard (MaxDAT): | dat15
transmissionWindowSize: | tw32
timerRST: | tr500
max_RST (MaxRST): | rst1
| pollingInfo:
timerPollProhibit: | tpp200
timerPoll: | tp200
poll_PDU: | Omit
poll_SDU: | sdu1
lastTransmissionPDU_Poll: | true
lastRetransmissionPDU_Poll: | true
pollWindow: | pw99
timerPollPeriodic: | Omit
| rB_LogCH_Mapping:
uLlogicalChannelIdentity (LogicalChannelIdentity): | 3
dLlogicalChannelIdentity (LogicalChannelIdentity): | 3
logicalChannelType: | Omit
cn_DomainIdentity: | Omit

#### CRLC_Config_CNF

LLA |  | RRC | @ 00:00:10.220

| Channel ID: |  | Rb3
| Cell ID: |  | -1

| Message Details:
| CRLC_Config_CNF:
cellId: | -1
| routingInfo:
rB_Identity: | 3

#### CRLC_Config_REQ

RRC |  | LLA | @ 00:00:10.220

| Channel ID: |  | Rb4
| Cell ID: |  | -1

| Message Details:
| CRLC_Config_REQ:
cellId: | -1
| routingInfo:
rB_Identity: | 4
ratType: | fdd
| configMessage: (CrlcConfigReq)
| setup: (RBInfo)
| sS_rlc_Info:
| sS_ul_RLC_Mode: (DL_RLC_Mode)
| dl_AM_RLC_Mode:
inSequenceDelivery: | true
receivingWindowSize: | rw32
| dl_RLC_StatusInfo:
timerStatusProhibit: | tsp200
timerEPC: | Omit
missingPDU_Indicator: | true
timerStatusPeriodic: | Omit
| sS_dl_RLC_Mode:
dl_PayloadSize (PayloadSize): | 128
| dl_RLCModeInfo: (UL_RLC_Mode)
| ul_AM_RLC_Mode:
| transmissionRLC_Discard:
noDiscard (MaxDAT): | dat15
transmissionWindowSize: | tw32
timerRST: | tr500
max_RST (MaxRST): | rst1
| pollingInfo:
timerPollProhibit: | tpp200
timerPoll: | tp200
poll_PDU: | Omit
poll_SDU: | sdu1
lastTransmissionPDU_Poll: | true
lastRetransmissionPDU_Poll: | true
pollWindow: | pw99
timerPollPeriodic: | Omit
| rB_LogCH_Mapping:
uLlogicalChannelIdentity (LogicalChannelIdentity): | 4
dLlogicalChannelIdentity (LogicalChannelIdentity): | 4
logicalChannelType: | Omit
cn_DomainIdentity: | Omit

#### CRLC_Config_CNF

LLA |  | RRC | @ 00:00:10.240

| Channel ID: |  | Rb4
| Cell ID: |  | -1

| Message Details:
| CRLC_Config_CNF:
cellId: | -1
| routingInfo:
rB_Identity: | 4

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:10.240

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 27
bcch_ModificationTime: | Omit

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:10.250

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:10.250

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
noSegment: |

#### o_SIB_PER_Encoding

RRC |  | RRC | @ 00:00:10.250

| Category: |  | TSO

| Message Details:
| Inputs:
| SIB:
| sIB1: (SysInfoType1)
cn_CommonGSM_MAP_NAS_SysInfo (NAS_SystemInformationGSM_MAP): |
[0] | 00 | 01 |  |  |  |  |  |
| cn_DomainSysInfoList:
| CN_DomainSysInfo:
cn_DomainIdentity: | ps_domain
| cn_Type:
gsm_MAP (NAS_SystemInformationGSM_MAP): |
[0] | 05 | 00 |  |  |  |  |  |
cn_DRX_CycleLengthCoeff (CN_DRX_CycleLengthCoefficient): | 7
| CN_DomainSysInfo:
cn_DomainIdentity: | cs_domain
| cn_Type:
gsm_MAP (NAS_SystemInformationGSM_MAP): |
[0] | 01 | 01 |  |  |  |  |  |
cn_DRX_CycleLengthCoeff (CN_DRX_CycleLengthCoefficient): | 7
| ue_ConnTimersAndConstants:
t_301: | Omit
n_301: | Omit
t_302: | Omit
n_302: | Omit
t_304: | Omit
n_304: | Omit
t_305: | Omit
t_307: | Omit
t_308: | Omit
t_309: | Omit
t_310: | Omit
n_310: | Omit
t_311: | Omit
t_312: | Omit
n_312: | Omit
t_313: | Omit
n_313: | Omit
t_314: | Omit
t_315: | Omit
n_315: | Omit
t_316: | Omit
t_317: | Omit
| ue_IdleTimersAndConstants:
t_300: | ms4000
n_300: | 3
t_312: | 10
n_312: | s1
| v3a0NonCriticalExtensions: Omit
| Outputs:
BITSTRING: |
[0] | 11 | 00 | 01 | 00 | 00 | 00 | 00 | 00
[8] | 00 | 00 | 01 | 01 | 10 | 00 | 10 | 00
[16] | 00 | 10 | 10 | 00 | 00 | 00 | 00 | 10
[24] | 00 | 01 | 00 | 00 | 00 | 01 | 00 | 00
[32] | 00 | 01 | 01 | 00 | 00 | 00 | 00 | 00
[40] | 00 | 00 | 00 | 00 | 00 | 00 | 11 | 00
[48] | 01 | 11 | 01 | 00 | 00 |  |  |

#### o_SIB_PER_Encoding

RRC |  | RRC | @ 00:00:10.250

| Category: |  | TSO

| Message Details:
| Inputs:
| SIB:
| sIB2: (SysInfoType2)
| ura_IdentityList:
URA_Identity: | 0000000000000001
| nonCriticalExtensions: Omit
| Outputs:
BITSTRING: |
[0] | 00 | 00 | 00 | 00 | 00 | 00 | 00 | 00
[8] | 00 | 01 |  |  |  |  |  |

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:10.250

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 11
bcch_ModificationTime: | Omit

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:10.270

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:10.270

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
| completeSIB_List:
| CompleteSIBshort:
sib_Type: | systemInformationBlockType1
sib_Data_variable: | 1100010000000000000001011000100000101000000000100001000000010000000101000000000000000000000011000111010000
| CompleteSIBshort:
sib_Type: | systemInformationBlockType2
sib_Data_variable: | 00000000000000000001

#### o_SIB_PER_Encoding

RRC |  | RRC | @ 00:00:10.270

| Category: |  | TSO

| Message Details:
| Inputs:
| SIB:
| sIB2: (SysInfoType2)
| ura_IdentityList:
URA_Identity: | 0000000000000001
| nonCriticalExtensions: Omit
| Outputs:
BITSTRING: |
[0] | 00 | 00 | 00 | 00 | 00 | 00 | 00 | 00
[8] | 00 | 01 |  |  |  |  |  |

#### o_SIB_PER_Encoding

RRC |  | RRC | @ 00:00:10.270

| Category: |  | TSO

| Message Details:
| Inputs:
| SIB:
| sIB1: (SysInfoType1)
cn_CommonGSM_MAP_NAS_SysInfo (NAS_SystemInformationGSM_MAP): |
[0] | 00 | 01 |  |  |  |  |  |
| cn_DomainSysInfoList:
| CN_DomainSysInfo:
cn_DomainIdentity: | ps_domain
| cn_Type:
gsm_MAP (NAS_SystemInformationGSM_MAP): |
[0] | 05 | 00 |  |  |  |  |  |
cn_DRX_CycleLengthCoeff (CN_DRX_CycleLengthCoefficient): | 7
| CN_DomainSysInfo:
cn_DomainIdentity: | cs_domain
| cn_Type:
gsm_MAP (NAS_SystemInformationGSM_MAP): |
[0] | 01 | 01 |  |  |  |  |  |
cn_DRX_CycleLengthCoeff (CN_DRX_CycleLengthCoefficient): | 7
| ue_ConnTimersAndConstants:
t_301: | Omit
n_301: | Omit
t_302: | Omit
n_302: | Omit
t_304: | Omit
n_304: | Omit
t_305: | Omit
t_307: | Omit
t_308: | Omit
t_309: | Omit
t_310: | Omit
n_310: | Omit
t_311: | Omit
t_312: | Omit
n_312: | Omit
t_313: | Omit
n_313: | Omit
t_314: | Omit
t_315: | Omit
n_315: | Omit
t_316: | Omit
t_317: | Omit
| ue_IdleTimersAndConstants:
t_300: | ms4000
n_300: | 3
t_312: | 10
n_312: | s1
| v3a0NonCriticalExtensions: Omit
| Outputs:
BITSTRING: |
[0] | 11 | 00 | 01 | 00 | 00 | 00 | 00 | 00
[8] | 00 | 00 | 01 | 01 | 10 | 00 | 10 | 00
[16] | 00 | 10 | 10 | 00 | 00 | 00 | 00 | 10
[24] | 00 | 01 | 00 | 00 | 00 | 01 | 00 | 00
[32] | 00 | 01 | 01 | 00 | 00 | 00 | 00 | 00
[40] | 00 | 00 | 00 | 00 | 00 | 00 | 11 | 00
[48] | 01 | 11 | 01 | 00 | 00 |  |  |

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:10.270

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 11
bcch_ModificationTime: | Omit

#### PHY_DATA_REQ

MAC |  | PHY | @ 00:00:10.270

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCH
| CFN: |  | 12

| Message Details:
SIB repetition period: | 64
SIB position: | 54
SIB size: | 246
SIB (raw): |
[0] | 00 | 00 | 00 | 00 | 00 | 00 | 00 | 00
[8] | 00 | 00 | 00 | 00 | 00 | 00 | 00 | 00
[16] | 00 | 00 | 00 | 00 | 00 | 00 | 00 | 00
[24] | 00 | 00 | 00 | 00 | 00 | 00 | 00 | 00
| SIB (decoded):
| TB 0:
MAC SDU (246 bits): |
[0] | 00 | 00 | 00 | 00 | 00 | 00 | 00 | 00
[8] | 00 | 00 | 00 | 00 | 00 | 00 | 00 | 00
[16] | 00 | 00 | 00 | 00 | 00 | 00 | 00 | 00
[24] | 00 | 00 | 00 | 00 | 00 | 00 | 00 |

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:10.290

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:10.290

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
| completeSIB_List:
| CompleteSIBshort:
sib_Type: | systemInformationBlockType1
sib_Data_variable: | 1100010000000000000001011000100000101000000000100001000000010000000101000000000000000000000011000111010000
| CompleteSIBshort:
sib_Type: | systemInformationBlockType2
sib_Data_variable: | 00000000000000000001

#### o_SIB_PER_Encoding

RRC |  | RRC | @ 00:00:10.290

| Category: |  | TSO

| Message Details:
| Inputs:
| SIB:
| sIB3: (SysInfoType3)
sib4indicator: | true
cellIdentity: | 0000000000000000000000000000
| cellSelectReselectInfo: (CellSelectReselectInfoSIB_3_4)
| mappingInfo: Omit
| cellSelectQualityMeasure:
cpich_RSCP: |
| modeSpecificInfo:
| fdd:
s_Intrasearch (S_SearchQual): | 8
s_Intersearch (S_SearchQual): | 8
s_SearchHCS (S_SearchRXLEV): | Omit
| rat_List: (RAT_FDD_InfoList)
| RAT_FDD_Info:
rat_Identifier: | gsm
s_SearchRAT (S_SearchQual): | -16
s_HCS_RAT (S_SearchRXLEV): | Omit
s_Limit_SearchRAT (S_SearchQual): | 0
q_QualMin: | -24
q_RxlevMin: | -40
q_Hyst_l_S (Q_Hyst_S): | 2
t_Reselection_S: | 0
| hcs_ServingCellInformation: Omit
maxAllowedUL_TX_Power: | 21
| cellAccessRestriction:
| cellBarred:
notBarred: |
cellReservedForOperatorUse (ReservedIndicator): | notReserved
cellReservationExtension (ReservedIndicator): | notReserved
| accessClassBarredList:
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
| nonCriticalExtensions: Omit
| Outputs:
BITSTRING: |
[0] | 01 | 00 | 00 | 00 | 00 | 00 | 00 | 00
[8] | 00 | 00 | 00 | 00 | 00 | 00 | 00 | 00
[16] | 10 | 11 | 01 | 11 | 00 | 01 | 10 | 00
[24] | 00 | 00 | 00 | 00 | 00 | 01 | 00 | 00
[32] | 00 | 00 | 00 | 10 | 01 | 00 | 00 | 10
[40] | 00 | 00 | 01 | 00 | 01 | 11 | 11 | 11
[48] | 11 | 11 | 11 | 11 | 11 | 11 | 11 | 11

#### o_SIB_PER_Encoding

RRC |  | RRC | @ 00:00:10.290

| Category: |  | TSO

| Message Details:
| Inputs:
| SIB:
| sIB7: (SysInfoType7)
| modeSpecificInfo:
| fdd:
ul_Interference: | -100
| prach_Information_SIB5_List: (DynamicPersistenceLevelList)
DynamicPersistenceLevel: | 2
| prach_Information_SIB6_List: (DynamicPersistenceLevelList)
DynamicPersistenceLevel: | 2
expirationTimeFactor: | Omit
| nonCriticalExtensions: Omit
| Outputs:
BITSTRING: |
[0] | 10 | 00 | 00 | 10 | 10 | 00 | 00 | 00
[8] | 10 | 00 | 00 | 01 |  |  |  |

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:10.290

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 10
bcch_ModificationTime: | Omit

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:10.300

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:10.300

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
| completeSIB_List:
| CompleteSIBshort:
sib_Type: | systemInformationBlockType7
sib_Data_variable: | 100000101000000010000001
| CompleteSIBshort:
sib_Type: | systemInformationBlockType3
sib_Data_variable: | 0100000000000000000000000000000010110111000110000000000000010000000000100100001000000100011111111111111111111111

#### o_SIB_PER_Encoding

RRC |  | RRC | @ 00:00:10.300

| Category: |  | TSO

| Message Details:
| Inputs:
| SIB:
| sIB4: (SysInfoType4)
cellIdentity: | 0000000000000000000000000000
| cellSelectReselectInfo: (CellSelectReselectInfoSIB_3_4)
| mappingInfo: Omit
| cellSelectQualityMeasure:
cpich_RSCP: |
| modeSpecificInfo:
| fdd:
s_Intrasearch (S_SearchQual): | 8
s_Intersearch (S_SearchQual): | 8
s_SearchHCS (S_SearchRXLEV): | Omit
| rat_List: (RAT_FDD_InfoList)
| RAT_FDD_Info:
rat_Identifier: | gsm
s_SearchRAT (S_SearchQual): | -16
s_HCS_RAT (S_SearchRXLEV): | Omit
s_Limit_SearchRAT (S_SearchQual): | 0
q_QualMin: | -24
q_RxlevMin: | -40
q_Hyst_l_S (Q_Hyst_S): | 0
t_Reselection_S: | 0
| hcs_ServingCellInformation: Omit
maxAllowedUL_TX_Power: | 21
| cellAccessRestriction:
| cellBarred:
notBarred: |
cellReservedForOperatorUse (ReservedIndicator): | notReserved
cellReservationExtension (ReservedIndicator): | notReserved
| accessClassBarredList: Omit
| nonCriticalExtensions: Omit
| Outputs:
BITSTRING: |
[0] | 00 | 00 | 00 | 00 | 00 | 00 | 00 | 00
[8] | 00 | 00 | 00 | 00 | 00 | 00 | 00 | 01
[16] | 01 | 10 | 11 | 10 | 00 | 11 | 00 | 00
[24] | 00 | 00 | 00 | 00 | 00 | 10 | 00 | 00
[32] | 00 | 00 | 01 | 00 | 10 | 00 | 00 | 00
[40] | 00 | 00 | 10 | 00 | 11 | 10 | 11 | 1

#### o_SIB_PER_Encoding

RRC |  | RRC | @ 00:00:10.300

| Category: |  | TSO

| Message Details:
| Inputs:
| SIB:
| sIB7: (SysInfoType7)
| modeSpecificInfo:
| fdd:
ul_Interference: | -100
| prach_Information_SIB5_List: (DynamicPersistenceLevelList)
DynamicPersistenceLevel: | 2
| prach_Information_SIB6_List: (DynamicPersistenceLevelList)
DynamicPersistenceLevel: | 2
expirationTimeFactor: | Omit
| nonCriticalExtensions: Omit
| Outputs:
BITSTRING: |
[0] | 10 | 00 | 00 | 10 | 10 | 00 | 00 | 00
[8] | 10 | 00 | 00 | 01 |  |  |  |

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:10.300

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 26
bcch_ModificationTime: | Omit

#### PHY_DATA_REQ

MAC |  | PHY | @ 00:00:10.310

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCH
| CFN: |  | 16

| Message Details:
SIB repetition period: | 64
SIB position: | 22
SIB size: | 246
SIB (raw): |
[0] | 00 | 0E | 21 | 69 | C4 | 00 | 05 | 88
[8] | 28 | 02 | 10 | 10 | 14 | 00 | 00 | 0C
[16] | 74 | 04 | 26 | 00 | 00 | 20 | 00 | 00
[24] | 00 | 00 | 00 | 00 | 00 | 00 | 00 | 00
| SIB (decoded):
| TB 0:
MAC SDU (246 bits): |
[0] | 00 | 0E | 21 | 69 | C4 | 00 | 05 | 88
[8] | 28 | 02 | 10 | 10 | 14 | 00 | 00 | 0C
[16] | 74 | 04 | 26 | 00 | 00 | 20 | 00 | 00
[24] | 00 | 00 | 00 | 00 | 00 | 00 | 00 |

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:10.320

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:10.320

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
| completeSIB_List:
| CompleteSIBshort:
sib_Type: | systemInformationBlockType7
sib_Data_variable: | 100000101000000010000001
| CompleteSIBshort:
sib_Type: | systemInformationBlockType4
sib_Data_variable: | 00000000000000000000000000000001011011100011000000000000001000000000010010000000000010001110111

#### PHY_DATA_REQ

MAC |  | PHY | @ 00:00:10.330

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCH
| CFN: |  | 18

| Message Details:
SIB repetition period: | 64
SIB position: | 22
SIB size: | 246
SIB (raw): |
[0] | 00 | 0E | 21 | 69 | C4 | 00 | 05 | 88
[8] | 28 | 02 | 10 | 10 | 14 | 00 | 00 | 0C
[16] | 74 | 04 | 26 | 00 | 00 | 20 | 00 | 00
[24] | 00 | 00 | 00 | 00 | 00 | 00 | 00 | 00
| SIB (decoded):
| TB 0:
MAC SDU (246 bits): |
[0] | 00 | 0E | 21 | 69 | C4 | 00 | 05 | 88
[8] | 28 | 02 | 10 | 10 | 14 | 00 | 00 | 0C
[16] | 74 | 04 | 26 | 00 | 00 | 20 | 00 | 00
[24] | 00 | 00 | 00 | 00 | 00 | 00 | 00 |

#### o_SIB_PER_Encoding

RRC |  | RRC | @ 00:00:10.350

| Category: |  | TSO

| Message Details:
| Inputs:
| SIB:
| sIB5: (SysInfoType5)
sib6indicator: | true
pich_PowerOffset: | -5
| modeSpecificInfo:
| fdd:
aich_PowerOffset: | -5
| primaryCCPCH_Info: Omit
| prach_SystemInformationList:
| PRACH_SystemInformation:
| prach_RACH_Info:
| modeSpecificInfo:
| fdd:
availableSignatures: | 0000000011111111
availableSF (SF_PRACH): | sfpr64
preambleScramblingCodeWordNumber: | 0
puncturingLimit: | pl1
availableSubChannelNumbers: | 111111111111
transportChannelIdentity: | 15
| rach_TransportFormatSet: (TransportFormatSet)
| commonTransChTFS:
| tti:
| tti20: (CommonDynamicTF_InfoList)
| CommonDynamicTF_Info:
| rlc_Size:
| fdd:
| octetModeRLC_SizeInfoType2:
sizeType1: | 15
| numberOfTbSizeList:
| NumberOfTransportBlocks:
one: |
| logicalChannelList:
configured: |
| CommonDynamicTF_Info:
| rlc_Size:
| fdd:
| octetModeRLC_SizeInfoType2:
sizeType2: | 3
| numberOfTbSizeList:
| NumberOfTransportBlocks:
one: |
| logicalChannelList:
configured: |
| semistaticTF_Information:
| channelCodingType:
convolutional (CodingRate): | half
rateMatchingAttribute: | 150
crc_Size: | crc16
| rach_TFCS: (TFCS)
| normalTFCI_Signalling: (ExplicitTFCS_Configuration)
| complete: (TFCS_ReconfAdd)
| ctfcSize:
| ctfc2Bit:
| :
ctfc2: | 0
| powerOffsetInformation:
| gainFactorInformation:
computedGainFactors (ReferenceTFC_ID): | 0
powerOffsetPp_m: | 0
| :
ctfc2: | 1
| powerOffsetInformation:
| gainFactorInformation:
| signalledGainFactors:
| modeSpecificInfo:
| fdd:
gainFactorBetaC (GainFactor): | 11
gainFactorBetaD (GainFactor): | 15
referenceTFC_ID: | 0
powerOffsetPp_m: | 0
| prach_Partitioning:
| fdd:
| ASCSetting_FDD:
| accessServiceClass_FDD: Omit
| ASCSetting_FDD:
| accessServiceClass_FDD:
availableSignatureStartIndex: | 0
availableSignatureEndIndex: | 7
assignedSubChannelNumber: | 1111
| ASCSetting_FDD:
| accessServiceClass_FDD: Omit
| ASCSetting_FDD:
| accessServiceClass_FDD:
availableSignatureStartIndex: | 0
availableSignatureEndIndex: | 7
assignedSubChannelNumber: | 1111
| ASCSetting_FDD:
| accessServiceClass_FDD: Omit
| ASCSetting_FDD:
| accessServiceClass_FDD:
availableSignatureStartIndex: | 0
availableSignatureEndIndex: | 7
assignedSubChannelNumber: | 1111
| ASCSetting_FDD:
| accessServiceClass_FDD: Omit
| ASCSetting_FDD:
| accessServiceClass_FDD:
availableSignatureStartIndex: | 0
availableSignatureEndIndex: | 7
assignedSubChannelNumber: | 1111
| persistenceScalingFactorList:
PersistenceScalingFactor: | psf0_9
PersistenceScalingFactor: | psf0_9
PersistenceScalingFactor: | psf0_9
PersistenceScalingFactor: | psf0_9
PersistenceScalingFactor: | psf0_9
PersistenceScalingFactor: | psf0_9
| ac_To_ASC_MappingTable:
AC_To_ASC_Mapping: | 6
AC_To_ASC_Mapping: | 5
AC_To_ASC_Mapping: | 4
AC_To_ASC_Mapping: | 3
AC_To_ASC_Mapping: | 2
AC_To_ASC_Mapping: | 1
AC_To_ASC_Mapping: | 0
| modeSpecificInfo:
| fdd:
primaryCPICH_TX_Power: | 31
constantValue: | -10
| prach_PowerOffset:
powerRampStep: | 3
preambleRetransMax: | 4
| rach_TransmissionParameters:
mmax: | 2
nb01Min (NB01): | 3
nb01Max (NB01): | 10
| aich_Info:
channelisationCode256: | 3
sttd_Indicator: | false
aich_TransmissionTiming: | e0
| sCCPCH_SystemInformationList:
| SCCPCH_SystemInformation:
| secondaryCCPCH_Info:
| modeSpecificInfo:
| fdd:
dummy1 (PCPICH_UsageForChannelEst): | mayBeUsed
| dummy2: (SecondaryCPICH_Info) Omit
secondaryScramblingCode: | Omit
sttd_Indicator: | false
| sf_AndCodeNumber: (SF256_AndCodeNumber)
sf64: | 1
pilotSymbolExistence: | false
tfci_Existence: | true
positionFixedOrFlexible: | flexible
timingOffset: | 0
| tfcs:
| normalTFCI_Signalling: (ExplicitTFCS_Configuration)
| complete: (TFCS_ReconfAdd)
| ctfcSize:
| ctfc4Bit:
| :
ctfc4: | 0
| powerOffsetInformation: Omit
| :
ctfc4: | 1
| powerOffsetInformation: Omit
| :
ctfc4: | 2
| powerOffsetInformation: Omit
| :
ctfc4: | 3
| powerOffsetInformation: Omit
| :
ctfc4: | 4
| powerOffsetInformation: Omit
| :
ctfc4: | 5
| powerOffsetInformation: Omit
| :
ctfc4: | 6
| powerOffsetInformation: Omit
| :
ctfc4: | 8
| powerOffsetInformation: Omit
| fach_PCH_InformationList:
| FACH_PCH_Information:
| transportFormatSet:
| commonTransChTFS:
| tti:
| tti10: (CommonDynamicTF_InfoList)
| CommonDynamicTF_Info:
| rlc_Size:
| fdd:
| octetModeRLC_SizeInfoType2:
sizeType1: | 24
| numberOfTbSizeList:
| NumberOfTransportBlocks:
zero: |
| NumberOfTransportBlocks:
one: |
| logicalChannelList:
allSizes: |
| semistaticTF_Information:
| channelCodingType:
convolutional (CodingRate): | half
rateMatchingAttribute: | 230
crc_Size: | crc16
transportChannelIdentity: | 12
ctch_Indicator: | false
| FACH_PCH_Information:
| transportFormatSet:
| commonTransChTFS:
| tti:
| tti10: (CommonDynamicTF_InfoList)
| CommonDynamicTF_Info:
| rlc_Size:
| fdd:
| octetModeRLC_SizeInfoType2:
sizeType1: | 15
| numberOfTbSizeList:
| NumberOfTransportBlocks:
zero: |
| NumberOfTransportBlocks:
one: |
| NumberOfTransportBlocks:
small: | 2
| logicalChannelList:
allSizes: |
| semistaticTF_Information:
| channelCodingType:
convolutional (CodingRate): | half
rateMatchingAttribute: | 220
crc_Size: | crc16
transportChannelIdentity: | 13
ctch_Indicator: | false
| FACH_PCH_Information:
| transportFormatSet:
| commonTransChTFS:
| tti:
| tti10: (CommonDynamicTF_InfoList)
| CommonDynamicTF_Info:
| rlc_Size:
| fdd:
| octetModeRLC_SizeInfoType2:
sizeType2: | 3
| numberOfTbSizeList:
| NumberOfTransportBlocks:
zero: |
| NumberOfTransportBlocks:
one: |
| logicalChannelList:
allSizes: |
| semistaticTF_Information:
| channelCodingType:
turbo: |
rateMatchingAttribute: | 130
crc_Size: | crc16
transportChannelIdentity: | 14
ctch_Indicator: | false
| pich_Info:
| fdd:
channelisationCode256: | 2
pi_CountPerFrame: | e18
sttd_Indicator: | false
| cbs_DRX_Level1Information: Omit
| nonCriticalExtensions: Omit
| Outputs:
BITSTRING: |
[0] | 00 | 01 | 01 | 01 | 01 | 00 | 01 | 00
[8] | 00 | 11 | 11 | 10 | 00 | 00 | 00 | 00
[16] | 11 | 11 | 11 | 11 | 01 | 00 | 00 | 11
[24] | 11 | 11 | 11 | 11 | 11 | 11 | 11 | 01
[32] | 11 | 01 | 00 | 10 | 00 | 01 | 00 | 00
[40] | 11 | 11 | 00 | 00 | 00 | 10 | 10 | 01
[48] | 00 | 00 | 11 | 00 | 00 | 00 | 10 | 10
[56] | 10 | 10 | 01 | 01 | 01 | 01 | 10 | 00
[64] | 00 | 00 | 00 | 00 | 00 | 00 | 11 | 00
[72] | 11 | 00 | 01 | 01 | 10 | 11 | 01 | 01
[80] | 01 | 11 | 11 | 10 | 00 | 10 | 10 | 11
[88] | 10 | 10 | 00 | 00 | 11 | 11 | 11 | 10
[96] | 10 | 00 | 00 | 11 | 11 | 11 | 10 | 10
[104] | 00 | 00 | 11 | 11 | 11 | 10 | 10 | 00
[112] | 00 | 11 | 11 | 11 | 11 | 01 | 00 | 00
[120] | 00 | 00 | 00 | 00 | 00 | 00 | 00 | 11
[128] | 01 | 01 | 10 | 00 | 11 | 01 | 00 | 01
[136] | 00 | 00 | 11 | 11 | 11 | 01 | 00 | 11
[144] | 10 | 01 | 01 | 00 | 00 | 01 | 10 | 00
[152] | 01 | 00 | 00 | 11 | 00 | 10 | 10 | 00
[160] | 00 | 00 | 11 | 00 | 00 | 00 | 11 | 10
[168] | 00 | 00 | 01 | 00 | 00 | 00 | 01 | 01
[176] | 10 | 00 | 00 | 10 | 00 | 00 | 00 | 11
[184] | 10 | 00 | 00 | 00 | 00 | 10 | 00 | 10
[192] | 00 | 01 | 10 | 01 | 00 | 00 | 10 | 10
[200] | 01 | 10 | 01 | 00 | 00 | 10 | 10 | 00
[208] | 00 | 00 | 00 | 00 | 11 | 00 | 00 | 00
[216] | 01 | 00 | 01 | 00 | 01 | 01 | 11 | 00
[224] | 10 | 10 | 11 | 01 | 01 | 10 | 10 | 00
[232] | 00 | 00 | 00 | 00 | 01 | 11 | 10 | 00
[240] | 10 | 00 | 01 | 10 | 00 | 00 | 00 | 01
[248] | 01 | 10 | 11 | 01 | 10 | 11 | 01 | 10
[256] | 00 | 10 | 00 | 00 | 00 | 00 | 01 | 00
[264] | 00 | 11 | 00 | 00 | 10 | 00 | 10 | 01
[272] | 01 | 00 | 00 | 00 | 10 | 11 | 01 | 10
[280] | 10 | 00 | 00 | 00 | 01 | 00 | 00 |

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:10.360

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 23
bcch_ModificationTime: | Omit

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:10.380

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:10.380

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
noSegment: |

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:10.380

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 19
bcch_ModificationTime: | Omit

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:10.390

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:10.390

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
| firstSegment:
sib_Type: | systemInformationBlockType5
seg_Count (SegCount): | 3
sib_Data_fixed: | 000101010100010000111110000000001111111101000011111111111111110111010010000100001111000000101001000011000000101010100101010110000000000000001100110001011011010101111110001010111010000011111110100000111111101000001111111010

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:10.390

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 21
bcch_ModificationTime: | Omit

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:10.410

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:10.410

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
| subsequentSegment:
sib_Type: | systemInformationBlockType5
segmentIndex: | 1
sib_Data_fixed: | 000011111111010000000000000000001101011000110100010000111111010011100101000001100001000011001010000000110000001110000001000000010110000010000000111000000000100010000110010000101001100100001010000000000011000000010001000101

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:10.410

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 22
bcch_ModificationTime: | Omit

#### PHY_DATA_REQ

MAC |  | PHY | @ 00:00:10.410

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCH
| CFN: |  | 26

| Message Details:
SIB repetition period: | 64
SIB position: | 20
SIB size: | 246
SIB (raw): |
[0] | 00 | 0E | 27 | 17 | 82 | 80 | 81 | 1B
[8] | 7A | 00 | 00 | 00 | 05 | B8 | C0 | 00
[16] | 80 | 12 | 10 | 23 | FF | FF | F8 | 00
[24] | 00 | 00 | 00 | 00 | 00 | 00 | 00 | 00
| SIB (decoded):
| TB 0:
MAC SDU (246 bits): |
[0] | 00 | 0E | 27 | 17 | 82 | 80 | 81 | 1B
[8] | 7A | 00 | 00 | 00 | 05 | B8 | C0 | 00
[16] | 80 | 12 | 10 | 23 | FF | FF | F8 | 00
[24] | 00 | 00 | 00 | 00 | 00 | 00 | 00 |

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:10.430

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:10.430

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
| lastSegmentShort:
sib_Type: | systemInformationBlockType5
segmentIndex: | 2
sib_Data_variable: | 1100101011010110100000000000011110001000011000000001011011011011011000100000000001000011000010001001010000001011011010000000010000

#### o_SIB_PER_Encoding

RRC |  | RRC | @ 00:00:10.430

| Category: |  | TSO

| Message Details:
| Inputs:
| SIB:
| sIB6: (SysInfoType6)
pich_PowerOffset: | -5
| modeSpecificInfo:
| fdd:
aich_PowerOffset: | -5
dummy (CSICH_PowerOffset): | Omit
| primaryCCPCH_Info: Omit
| prach_SystemInformationList: Omit
| sCCPCH_SystemInformationList: Omit
| cbs_DRX_Level1Information: Omit
| nonCriticalExtensions: Omit
| Outputs:
BITSTRING: |
[0] | 00 | 00 | 00 | 10 | 10 | 01 | 00 | 01

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:10.430

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 3
bcch_ModificationTime: | Omit

#### PHY_DATA_REQ

MAC |  | PHY | @ 00:00:10.430

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCH
| CFN: |  | 28

| Message Details:
SIB repetition period: | 64
SIB position: | 52
SIB size: | 246
SIB (raw): |
[0] | 00 | 0E | 27 | 17 | 82 | 80 | 81 | 22
[8] | F0 | 00 | 00 | 00 | 0B | 71 | 80 | 01
[16] | 00 | 24 | 00 | 47 | 70 | FF | F8 | 00
[24] | 00 | 00 | 00 | 00 | 00 | 00 | 00 | 00
| SIB (decoded):
| TB 0:
MAC SDU (246 bits): |
[0] | 00 | 0E | 27 | 17 | 82 | 80 | 81 | 22
[8] | F0 | 00 | 00 | 00 | 0B | 71 | 80 | 01
[16] | 00 | 24 | 00 | 47 | 70 | FF | F8 | 00
[24] | 00 | 00 | 00 | 00 | 00 | 00 | 00 |

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:10.440

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:10.440

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
| completeSIB_List:
| CompleteSIBshort:
sib_Type: | systemInformationBlockType6
sib_Data_variable: | 0000001010010001

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:10.440

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 5
bcch_ModificationTime: | Omit

#### PHY_DATA_REQ

MAC |  | PHY | @ 00:00:10.450

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCH
| CFN: |  | 30

| Message Details:
SIB repetition period: | 64
SIB position: | 46
SIB size: | 246
SIB (raw): |
[0] | 00 | 00 | 27 | 17 | 82 | 80 | 81 | 22
[8] | F0 | 00 | 00 | 00 | 0B | 71 | 80 | 01
[16] | 00 | 24 | 00 | 47 | 70 | FF | F8 | 00
[24] | 00 | 00 | 00 | 00 | 00 | 00 | 00 | 00
| SIB (decoded):
| TB 0:
MAC SDU (246 bits): |
[0] | 00 | 00 | 27 | 17 | 82 | 80 | 81 | 22
[8] | F0 | 00 | 00 | 00 | 0B | 71 | 80 | 01
[16] | 00 | 24 | 00 | 47 | 70 | FF | F8 | 00
[24] | 00 | 00 | 00 | 00 | 00 | 00 | 00 |

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:10.460

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:10.460

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
noSegment: |

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:10.460

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 6
bcch_ModificationTime: | Omit

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:10.470

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:10.470

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
noSegment: |

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:10.470

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 7
bcch_ModificationTime: | Omit

#### PHY_DATA_REQ

MAC |  | PHY | @ 00:00:10.470

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCH
| CFN: |  | 32

| Message Details:
SIB repetition period: | 64
SIB position: | 38
SIB size: | 246
SIB (raw): |
[0] | 00 | 02 | 52 | 15 | 44 | 3E | 00 | FF
[8] | 43 | FF | FD | D2 | 10 | F0 | 29 | 0C
[16] | 0A | A5 | 58 | 00 | 0C | C5 | B5 | 7E
[24] | 2B | A0 | FE | 83 | FA | 0F | E8 | 00
| SIB (decoded):
| TB 0:
MAC SDU (246 bits): |
[0] | 00 | 02 | 52 | 15 | 44 | 3E | 00 | FF
[8] | 43 | FF | FD | D2 | 10 | F0 | 29 | 0C
[16] | 0A | A5 | 58 | 00 | 0C | C5 | B5 | 7E
[24] | 2B | A0 | FE | 83 | FA | 0F | E8 |

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:10.490

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:10.490

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
noSegment: |

#### o_SIB_PER_Encoding

RRC |  | RRC | @ 00:00:10.490

| Category: |  | TSO

| Message Details:
| Inputs:
| SIB:
| sIB7: (SysInfoType7)
| modeSpecificInfo:
| fdd:
ul_Interference: | -100
| prach_Information_SIB5_List: (DynamicPersistenceLevelList)
DynamicPersistenceLevel: | 2
| prach_Information_SIB6_List: (DynamicPersistenceLevelList)
DynamicPersistenceLevel: | 2
expirationTimeFactor: | Omit
| nonCriticalExtensions: Omit
| Outputs:
BITSTRING: |
[0] | 10 | 00 | 00 | 10 | 10 | 00 | 00 | 00
[8] | 10 | 00 | 00 | 01 |  |  |  |

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:10.490

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 2
bcch_ModificationTime: | Omit

#### PHY_DATA_REQ

MAC |  | PHY | @ 00:00:10.490

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCH
| CFN: |  | 34

| Message Details:
SIB repetition period: | 64
SIB position: | 42
SIB size: | 246
SIB (raw): |
[0] | 00 | 04 | 50 | 0F | F4 | 00 | 00 | D6
[8] | 34 | 43 | F4 | E5 | 06 | 10 | CA | 03
[16] | 03 | 81 | 01 | 60 | 80 | E0 | 08 | 86
[24] | 42 | 99 | 0A | 00 | 30 | 11 | 14 | 00
| SIB (decoded):
| TB 0:
MAC SDU (246 bits): |
[0] | 00 | 04 | 50 | 0F | F4 | 00 | 00 | D6
[8] | 34 | 43 | F4 | E5 | 06 | 10 | CA | 03
[16] | 03 | 81 | 01 | 60 | 80 | E0 | 08 | 86
[24] | 42 | 99 | 0A | 00 | 30 | 11 | 14 |

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:10.500

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:10.500

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
| completeSIB_List:
| CompleteSIBshort:
sib_Type: | systemInformationBlockType7
sib_Data_variable: | 100000101000000010000001

#### o_SIB_PER_Encoding

RRC |  | RRC | @ 00:00:10.500

| Category: |  | TSO

| Message Details:
| Inputs:
| SIB:
| sIB7: (SysInfoType7)
| modeSpecificInfo:
| fdd:
ul_Interference: | -100
| prach_Information_SIB5_List: (DynamicPersistenceLevelList)
DynamicPersistenceLevel: | 2
| prach_Information_SIB6_List: (DynamicPersistenceLevelList)
DynamicPersistenceLevel: | 2
expirationTimeFactor: | Omit
| nonCriticalExtensions: Omit
| Outputs:
BITSTRING: |
[0] | 10 | 00 | 00 | 10 | 10 | 00 | 00 | 00
[8] | 10 | 00 | 00 | 01 |  |  |  |

#### o_SIB_PER_Encoding

RRC |  | RRC | @ 00:00:10.500

| Category: |  | TSO

| Message Details:
| Inputs:
| SIB:
| sIB3: (SysInfoType3)
sib4indicator: | true
cellIdentity: | 0000000000000000000000000000
| cellSelectReselectInfo: (CellSelectReselectInfoSIB_3_4)
| mappingInfo: Omit
| cellSelectQualityMeasure:
cpich_RSCP: |
| modeSpecificInfo:
| fdd:
s_Intrasearch (S_SearchQual): | 8
s_Intersearch (S_SearchQual): | 8
s_SearchHCS (S_SearchRXLEV): | Omit
| rat_List: (RAT_FDD_InfoList)
| RAT_FDD_Info:
rat_Identifier: | gsm
s_SearchRAT (S_SearchQual): | -16
s_HCS_RAT (S_SearchRXLEV): | Omit
s_Limit_SearchRAT (S_SearchQual): | 0
q_QualMin: | -24
q_RxlevMin: | -40
q_Hyst_l_S (Q_Hyst_S): | 2
t_Reselection_S: | 0
| hcs_ServingCellInformation: Omit
maxAllowedUL_TX_Power: | 21
| cellAccessRestriction:
| cellBarred:
notBarred: |
cellReservedForOperatorUse (ReservedIndicator): | notReserved
cellReservationExtension (ReservedIndicator): | notReserved
| accessClassBarredList:
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
| nonCriticalExtensions: Omit
| Outputs:
BITSTRING: |
[0] | 01 | 00 | 00 | 00 | 00 | 00 | 00 | 00
[8] | 00 | 00 | 00 | 00 | 00 | 00 | 00 | 00
[16] | 10 | 11 | 01 | 11 | 00 | 01 | 10 | 00
[24] | 00 | 00 | 00 | 00 | 00 | 01 | 00 | 00
[32] | 00 | 00 | 00 | 10 | 01 | 00 | 00 | 10
[40] | 00 | 00 | 01 | 00 | 01 | 11 | 11 | 11
[48] | 11 | 11 | 11 | 11 | 11 | 11 | 11 | 11

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:10.500

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 10
bcch_ModificationTime: | Omit

#### PHY_DATA_REQ

MAC |  | PHY | @ 00:00:10.510

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCH
| CFN: |  | 36

| Message Details:
SIB repetition period: | 64
SIB position: | 44
SIB size: | 246
SIB (raw): |
[0] | 00 | 06 | 51 | 81 | CA | D6 | 80 | 07
[8] | 88 | 60 | 16 | DB | 62 | 00 | 43 | 08
[16] | 94 | 0B | 68 | 04 | 00 | E0 | 08 | 86
[24] | 42 | 99 | 0A | 00 | 30 | 11 | 14 | 00
| SIB (decoded):
| TB 0:
MAC SDU (246 bits): |
[0] | 00 | 06 | 51 | 81 | CA | D6 | 80 | 07
[8] | 88 | 60 | 16 | DB | 62 | 00 | 43 | 08
[16] | 94 | 0B | 68 | 04 | 00 | E0 | 08 | 86
[24] | 42 | 99 | 0A | 00 | 30 | 11 | 14 |

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:10.520

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:10.520

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
| completeSIB_List:
| CompleteSIBshort:
sib_Type: | systemInformationBlockType7
sib_Data_variable: | 100000101000000010000001
| CompleteSIBshort:
sib_Type: | systemInformationBlockType3
sib_Data_variable: | 0100000000000000000000000000000010110111000110000000000000010000000000100100001000000100011111111111111111111111

#### o_SIB_PER_Encoding

RRC |  | RRC | @ 00:00:10.520

| Category: |  | TSO

| Message Details:
| Inputs:
| SIB:
| sIB18: (SysInfoType18)
| idleModePLMNIdentities: (PLMNIdentitiesOfNeighbourCells)
| plmnsOfIntraFreqCellsList: Omit
| plmnsOfInterFreqCellsList: Omit
| plmnsOfInterRATCellsList: Omit
| connectedModePLMNIdentities: (PLMNIdentitiesOfNeighbourCells) Omit
| nonCriticalExtensions: Omit
| Outputs:
BITSTRING: |
[0] | 10 | 00 | 00 |  |  |  |  |

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:10.520

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 18
bcch_ModificationTime: | Omit

#### PHY_DATA_REQ

MAC |  | PHY | @ 00:00:10.530

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCH
| CFN: |  | 38

| Message Details:
SIB repetition period: | 64
SIB position: | 6
SIB size: | 246
SIB (raw): |
[0] | 00 | 0E | 06 | 0F | 02 | 91 | 80 | 07
[8] | 88 | 60 | 16 | DB | 62 | 00 | 43 | 08
[16] | 94 | 0B | 68 | 04 | 00 | E0 | 08 | 86
[24] | 42 | 99 | 0A | 00 | 30 | 11 | 14 | 00
| SIB (decoded):
| TB 0:
MAC SDU (246 bits): |
[0] | 00 | 0E | 06 | 0F | 02 | 91 | 80 | 07
[8] | 88 | 60 | 16 | DB | 62 | 00 | 43 | 08
[16] | 94 | 0B | 68 | 04 | 00 | E0 | 08 | 86
[24] | 42 | 99 | 0A | 00 | 30 | 11 | 14 |

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:10.540

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:10.540

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
| completeSIB_List:
| CompleteSIBshort:
sib_Type: | systemInformationBlockType7
sib_Data_variable: | 100000101000000010000001
| CompleteSIBshort:
sib_Type: | systemInformationBlockType18
sib_Data_variable: | 100000

#### o_SIB_PER_Encoding

RRC |  | RRC | @ 00:00:10.540

| Category: |  | TSO

| Message Details:
| Inputs:
| SIB:
| sIB4: (SysInfoType4)
cellIdentity: | 0000000000000000000000000000
| cellSelectReselectInfo: (CellSelectReselectInfoSIB_3_4)
| mappingInfo: Omit
| cellSelectQualityMeasure:
cpich_RSCP: |
| modeSpecificInfo:
| fdd:
s_Intrasearch (S_SearchQual): | 8
s_Intersearch (S_SearchQual): | 8
s_SearchHCS (S_SearchRXLEV): | Omit
| rat_List: (RAT_FDD_InfoList)
| RAT_FDD_Info:
rat_Identifier: | gsm
s_SearchRAT (S_SearchQual): | -16
s_HCS_RAT (S_SearchRXLEV): | Omit
s_Limit_SearchRAT (S_SearchQual): | 0
q_QualMin: | -24
q_RxlevMin: | -40
q_Hyst_l_S (Q_Hyst_S): | 0
t_Reselection_S: | 0
| hcs_ServingCellInformation: Omit
maxAllowedUL_TX_Power: | 21
| cellAccessRestriction:
| cellBarred:
notBarred: |
cellReservedForOperatorUse (ReservedIndicator): | notReserved
cellReservationExtension (ReservedIndicator): | notReserved
| accessClassBarredList: Omit
| nonCriticalExtensions: Omit
| Outputs:
BITSTRING: |
[0] | 00 | 00 | 00 | 00 | 00 | 00 | 00 | 00
[8] | 00 | 00 | 00 | 00 | 00 | 00 | 00 | 01
[16] | 01 | 10 | 11 | 10 | 00 | 11 | 00 | 00
[24] | 00 | 00 | 00 | 00 | 00 | 10 | 00 | 00
[32] | 00 | 00 | 01 | 00 | 10 | 00 | 00 | 00
[40] | 00 | 00 | 10 | 00 | 11 | 10 | 11 | 1

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:10.540

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 26
bcch_ModificationTime: | Omit

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:10.550

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:10.550

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
| completeSIB_List:
| CompleteSIBshort:
sib_Type: | systemInformationBlockType7
sib_Data_variable: | 100000101000000010000001
| CompleteSIBshort:
sib_Type: | systemInformationBlockType4
sib_Data_variable: | 00000000000000000000000000000001011011100011000000000000001000000000010010000000000010001110111

#### PHY_DATA_REQ

MAC |  | PHY | @ 00:00:10.550

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCH
| CFN: |  | 40

| Message Details:
SIB repetition period: | 64
SIB position: | 10
SIB size: | 246
SIB (raw): |
[0] | 00 | 00 | 06 | 0F | 02 | 91 | 80 | 07
[8] | 88 | 60 | 16 | DB | 62 | 00 | 43 | 08
[16] | 94 | 0B | 68 | 04 | 00 | E0 | 08 | 86
[24] | 42 | 99 | 0A | 00 | 30 | 11 | 14 | 00
| SIB (decoded):
| TB 0:
MAC SDU (246 bits): |
[0] | 00 | 00 | 06 | 0F | 02 | 91 | 80 | 07
[8] | 88 | 60 | 16 | DB | 62 | 00 | 43 | 08
[16] | 94 | 0B | 68 | 04 | 00 | E0 | 08 | 86
[24] | 42 | 99 | 0A | 00 | 30 | 11 | 14 |

#### o_SIB_PER_Encoding

RRC |  | RRC | @ 00:00:10.570

| Category: |  | TSO

| Message Details:
| Inputs:
| SIB:
| sIB11: (SysInfoType11)
sib12indicator: | true
| fach_MeasurementOccasionInfo: Omit
| measurementControlSysInfo:
| use_of_HCS:
| hcs_not_used:
| cellSelectQualityMeasure:
| cpich_RSCP:
| intraFreqMeasurementSysInfo: (IntraFreqMeasurementSysInfo_RSCP)
intraFreqMeasurementID (MeasurementIdentity): | Omit
| intraFreqCellInfoSI_List: (IntraFreqCellInfoSI_List_RSCP)
| removedIntraFreqCellList: Omit
| newIntraFreqCellList: (NewIntraFreqCellSI_List_RSCP)
| NewIntraFreqCellSI_RSCP:
intraFreqCellID: | 0
| cellInfo: (CellInfoSI_RSCP)
cellIndividualOffset: | Omit
| referenceTimeDifferenceToCell: Omit
| modeSpecificInfo:
| fdd:
| primaryCPICH_Info:
primaryScramblingCode: | 100
primaryCPICH_TX_Power: | Omit
readSFN_Indicator: | false
tx_DiversityIndicator: | false
| cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP) Omit
| NewIntraFreqCellSI_RSCP:
intraFreqCellID: | 1
| cellInfo: (CellInfoSI_RSCP)
cellIndividualOffset: | Omit
| referenceTimeDifferenceToCell: Omit
| modeSpecificInfo:
| fdd:
| primaryCPICH_Info:
primaryScramblingCode: | 150
primaryCPICH_TX_Power: | Omit
readSFN_Indicator: | true
tx_DiversityIndicator: | false
| cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP) Omit
| NewIntraFreqCellSI_RSCP:
intraFreqCellID: | 2
| cellInfo: (CellInfoSI_RSCP)
cellIndividualOffset: | Omit
| referenceTimeDifferenceToCell: Omit
| modeSpecificInfo:
| fdd:
| primaryCPICH_Info:
primaryScramblingCode: | 200
primaryCPICH_TX_Power: | Omit
readSFN_Indicator: | true
tx_DiversityIndicator: | false
| cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP) Omit
| NewIntraFreqCellSI_RSCP:
intraFreqCellID: | 6
| cellInfo: (CellInfoSI_RSCP)
cellIndividualOffset: | Omit
| referenceTimeDifferenceToCell: Omit
| modeSpecificInfo:
| fdd:
| primaryCPICH_Info:
primaryScramblingCode: | 400
primaryCPICH_TX_Power: | Omit
readSFN_Indicator: | true
tx_DiversityIndicator: | false
| cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP) Omit
| NewIntraFreqCellSI_RSCP:
intraFreqCellID: | 7
| cellInfo: (CellInfoSI_RSCP)
cellIndividualOffset: | Omit
| referenceTimeDifferenceToCell: Omit
| modeSpecificInfo:
| fdd:
| primaryCPICH_Info:
primaryScramblingCode: | 450
primaryCPICH_TX_Power: | Omit
readSFN_Indicator: | true
tx_DiversityIndicator: | false
| cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP) Omit
| intraFreqMeasQuantity:
filterCoefficient: | Omit
| modeSpecificInfo:
| fdd:
intraFreqMeasQuantity_FDD: | cpich_RSCP
| intraFreqReportingQuantityForRACH: Omit
maxReportedCellsOnRACH: | Omit
| reportingInfoForCellDCH:
| intraFreqReportingQuantity:
| activeSetReportingQuantities: (CellReportingQuantities)
dummy (SFN_SFN_OTD_Type): | noReport
cellIdentity_reportingIndicator: | true
cellSynchronisationInfoReportingIndicator: | false
| modeSpecificInfo:
| fdd:
cpich_Ec_N0_reportingIndicator: | false
cpich_RSCP_reportingIndicator: | true
pathloss_reportingIndicator: | false
| monitoredSetReportingQuantities: (CellReportingQuantities)
dummy (SFN_SFN_OTD_Type): | noReport
cellIdentity_reportingIndicator: | true
cellSynchronisationInfoReportingIndicator: | true
| modeSpecificInfo:
| fdd:
cpich_Ec_N0_reportingIndicator: | false
cpich_RSCP_reportingIndicator: | true
pathloss_reportingIndicator: | false
| detectedSetReportingQuantities: (CellReportingQuantities) Omit
| measurementReportingMode:
measurementReportTransferMode (TransferMode): | acknowledgedModeRLC
periodicalOrEventTrigger: | eventTrigger
| reportCriteria: (CellDCH_ReportCriteria)
| intraFreqReportingCriteria:
| eventCriteriaList: (IntraFreqEventCriteriaList)
| IntraFreqEventCriteria:
| event: (IntraFreqEvent)
| e1a: (Event1a)
triggeringCondition (TriggeringCondition2): | monitoredSetCellsOnly
reportingRange: | 5
| forbiddenAffectCellList: Omit
w: | 1
reportDeactivationThreshold: | t2
reportingAmount: | ra4
reportingInterval: | ri4
hysteresis: | 0
timeToTrigger: | ttt640
| reportingCellStatus:
withinActiveAndOrMonitoredUsedFreq (MaxNumberOfReportingCellsType1): | e3
| IntraFreqEventCriteria:
| event: (IntraFreqEvent)
| e1b: (Event1b)
triggeringCondition (TriggeringCondition1): | activeSetCellsOnly
reportingRange: | 5
| forbiddenAffectCellList: Omit
w: | 1
hysteresis: | 0
timeToTrigger: | ttt640
| reportingCellStatus:
withinActiveAndOrMonitoredUsedFreq (MaxNumberOfReportingCellsType1): | e3
| IntraFreqEventCriteria:
| event: (IntraFreqEvent)
| e1c: (Event1c)
replacementActivationThreshold: | t3
reportingAmount: | ra4
reportingInterval: | ri4
hysteresis: | 0
timeToTrigger: | ttt640
| reportingCellStatus:
withinActiveAndOrMonitoredUsedFreq (MaxNumberOfReportingCellsType1): | e3
| interFreqMeasurementSysInfo: (InterFreqMeasurementSysInfo_RSCP)
| interFreqCellInfoSI_List: (InterFreqCellInfoSI_List_RSCP)
| removedInterFreqCellList: Omit
| newInterFreqCellList: (NewInterFreqCellSI_List_RSCP)
| NewInterFreqCellSI_RSCP:
interFreqCellID: | 3
| frequencyInfo:
| modeSpecificInfo:
| fdd: (FrequencyInfoFDD)
uarfcn_UL (UARFCN): | Omit
uarfcn_DL (UARFCN): | 10837
| cellInfo: (CellInfoSI_RSCP)
cellIndividualOffset: | Omit
| referenceTimeDifferenceToCell: Omit
| modeSpecificInfo:
| fdd:
| primaryCPICH_Info:
primaryScramblingCode: | 250
primaryCPICH_TX_Power: | Omit
readSFN_Indicator: | false
tx_DiversityIndicator: | false
| cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP) Omit
| NewInterFreqCellSI_RSCP:
interFreqCellID: | 4
| frequencyInfo: Omit
| cellInfo: (CellInfoSI_RSCP)
cellIndividualOffset: | Omit
| referenceTimeDifferenceToCell: Omit
| modeSpecificInfo:
| fdd:
| primaryCPICH_Info:
primaryScramblingCode: | 300
primaryCPICH_TX_Power: | Omit
readSFN_Indicator: | false
tx_DiversityIndicator: | false
| cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP) Omit
| NewInterFreqCellSI_RSCP:
interFreqCellID: | 5
| frequencyInfo: Omit
| cellInfo: (CellInfoSI_RSCP)
cellIndividualOffset: | Omit
| referenceTimeDifferenceToCell: Omit
| modeSpecificInfo:
| fdd:
| primaryCPICH_Info:
primaryScramblingCode: | 350
primaryCPICH_TX_Power: | Omit
readSFN_Indicator: | false
tx_DiversityIndicator: | false
| cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP) Omit
| interRATMeasurementSysInfo: (InterRATMeasurementSysInfo_B) Omit
| trafficVolumeMeasSysInfo: Omit
| dummy: (UE_InternalMeasurementSysInfo) Omit
| nonCriticalExtensions: Omit
| Outputs:
BITSTRING: |
[0] | 00 | 10 | 00 | 00 | 11 | 01 | 10 | 01
[8] | 00 | 01 | 00 | 10 | 00 | 00 | 00 | 00
[16] | 10 | 00 | 11 | 00 | 10 | 00 | 01 | 00
[24] | 00 | 10 | 00 | 01 | 00 | 10 | 01 | 01
[32] | 10 | 10 | 10 | 00 | 10 | 00 | 00 | 10
[40] | 01 | 10 | 01 | 00 | 01 | 01 | 00 | 11
[48] | 00 | 00 | 01 | 01 | 10 | 01 | 00 | 00
[56] | 10 | 10 | 01 | 11 | 00 | 00 | 10 | 11
[64] | 10 | 00 | 01 | 01 | 00 | 00 | 10 | 00
[72] | 10 | 00 | 10 | 00 | 11 | 00 | 10 | 01
[80] | 01 | 01 | 01 | 00 | 00 | 00 | 01 | 00
[88] | 10 | 10 | 00 | 01 | 01 | 00 | 10 | 10
[96] | 10 | 00 | 01 | 10 | 00 | 01 | 00 | 10
[104] | 10 | 00 | 10 | 00 | 00 | 10 | 10 | 00
[112] | 01 | 00 | 00 | 11 | 00 | 00 | 10 | 01
[120] | 01 | 00 | 10 | 01 | 10 | 10 | 10 | 10
[128] | 00 | 01 | 10 | 00 | 01 | 00 | 10 | 10
[136] | 10 | 00 | 10 | 11 | 00 | 01 | 10 | 01
[144] | 01 | 01 | 00 | 10 | 10 | 10 | 10 | 00
[152] | 01 | 00 | 11 | 11 | 10 | 10 | 00 | 10
[160] | 00 | 10 | 00 | 00 | 01 | 01 | 00 | 10
[168] | 11 | 00 | 00 | 10 | 00 | 10 | 10 | 00
[176] | 01 | 01 | 01 | 01 | 11 | 10 | 00 |

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:10.580

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 31
bcch_ModificationTime: | Omit

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:10.600

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:10.600

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
noSegment: |

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:10.600

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 29
bcch_ModificationTime: | Omit

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:10.610

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:10.610

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
| firstSegment:
sib_Type: | systemInformationBlockType11
seg_Count (SegCount): | 2
sib_Data_fixed: | 001000001101100100010010000000001000110010000100001000010010010110101000100000100110010001010011000001011001000010100111000010111000010100001000100010001100100101010100000001001010000101001010100001100001001010001000001010

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:10.610

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 30
bcch_ModificationTime: | Omit

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:10.630

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:10.630

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
| lastSegmentShort:
sib_Type: | systemInformationBlockType11
segmentIndex: | 1
sib_Data_variable: | 000100001100001001010010011010101000011000010010101000101100011001010100101010100001001111101000100010000001010010110000100010100001010101111000

#### o_SIB_PER_Encoding

RRC |  | RRC | @ 00:00:10.630

| Category: |  | TSO

| Message Details:
| Inputs:
| SIB:
| sIB12: (SysInfoType12)
| fach_MeasurementOccasionInfo: Omit
| measurementControlSysInfo:
| use_of_HCS:
| hcs_not_used:
| cellSelectQualityMeasure:
| cpich_RSCP:
| intraFreqMeasurementSysInfo: (IntraFreqMeasurementSysInfo_RSCP) Omit
| interFreqMeasurementSysInfo: (InterFreqMeasurementSysInfo_RSCP) Omit
| interRATMeasurementSysInfo: (InterRATMeasurementSysInfo_B) Omit
| trafficVolumeMeasSysInfo: Omit
| dummy: (UE_InternalMeasurementSysInfo) Omit
| nonCriticalExtensions: Omit
| Outputs:
BITSTRING: |
[0] | 00 | 00 | 00 | 00 | 0 |  |  |

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:10.630

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 13
bcch_ModificationTime: | Omit

#### PHY_DATA_REQ

MAC |  | PHY | @ 00:00:10.630

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCH
| CFN: |  | 48

| Message Details:
SIB repetition period: | 64
SIB position: | 12
SIB size: | 246
SIB (raw): |
[0] | 00 | 00 | 06 | 0F | 02 | 91 | 80 | 07
[8] | 88 | 60 | 16 | DB | 62 | 00 | 43 | 08
[16] | 94 | 0B | 68 | 04 | 00 | E0 | 08 | 86
[24] | 42 | 99 | 0A | 00 | 30 | 11 | 14 | 00
| SIB (decoded):
| TB 0:
MAC SDU (246 bits): |
[0] | 00 | 00 | 06 | 0F | 02 | 91 | 80 | 07
[8] | 88 | 60 | 16 | DB | 62 | 00 | 43 | 08
[16] | 94 | 0B | 68 | 04 | 00 | E0 | 08 | 86
[24] | 42 | 99 | 0A | 00 | 30 | 11 | 14 |

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:10.640

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:10.640

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
| completeSIB_List:
| CompleteSIBshort:
sib_Type: | systemInformationBlockType12
sib_Data_variable: | 000000000

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:10.640

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 14
bcch_ModificationTime: | Omit

#### PHY_DATA_REQ

MAC |  | PHY | @ 00:00:10.650

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCH
| CFN: |  | 50

| Message Details:
SIB repetition period: | 64
SIB position: | 14
SIB size: | 246
SIB (raw): |
[0] | 00 | 00 | 06 | 0F | 02 | 91 | 80 | 07
[8] | 88 | 60 | 16 | DB | 62 | 00 | 43 | 08
[16] | 94 | 0B | 68 | 04 | 00 | E0 | 08 | 86
[24] | 42 | 99 | 0A | 00 | 30 | 11 | 14 | 00
| SIB (decoded):
| TB 0:
MAC SDU (246 bits): |
[0] | 00 | 00 | 06 | 0F | 02 | 91 | 80 | 07
[8] | 88 | 60 | 16 | DB | 62 | 00 | 43 | 08
[16] | 94 | 0B | 68 | 04 | 00 | E0 | 08 | 86
[24] | 42 | 99 | 0A | 00 | 30 | 11 | 14 |

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:10.660

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:10.660

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
noSegment: |

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:10.660

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 15
bcch_ModificationTime: | Omit

#### PHY_DATA_REQ

MAC |  | PHY | @ 00:00:10.670

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCH
| CFN: |  | 52

| Message Details:
SIB repetition period: | 64
SIB position: | 4
SIB size: | 246
SIB (raw): |
[0] | 00 | 0E | 07 | 17 | 82 | 80 | 81 | 07
[8] | 88 | 60 | 16 | DB | 62 | 00 | 43 | 08
[16] | 94 | 0B | 68 | 04 | 00 | E0 | 08 | 86
[24] | 42 | 99 | 0A | 00 | 30 | 11 | 14 | 00
| SIB (decoded):
| TB 0:
MAC SDU (246 bits): |
[0] | 00 | 0E | 07 | 17 | 82 | 80 | 81 | 07
[8] | 88 | 60 | 16 | DB | 62 | 00 | 43 | 08
[16] | 94 | 0B | 68 | 04 | 00 | E0 | 08 | 86
[24] | 42 | 99 | 0A | 00 | 30 | 11 | 14 |

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:10.680

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:10.680

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
noSegment: |

#### o_SIB_PER_Encoding

RRC |  | RRC | @ 00:00:10.680

| Category: |  | TSO

| Message Details:
| Inputs:
| SIB:
| sIB18: (SysInfoType18)
| idleModePLMNIdentities: (PLMNIdentitiesOfNeighbourCells)
| plmnsOfIntraFreqCellsList: Omit
| plmnsOfInterFreqCellsList: Omit
| plmnsOfInterRATCellsList: Omit
| connectedModePLMNIdentities: (PLMNIdentitiesOfNeighbourCells) Omit
| nonCriticalExtensions: Omit
| Outputs:
BITSTRING: |
[0] | 10 | 00 | 00 |  |  |  |  |

#### o_SIB_PER_Encoding

RRC |  | RRC | @ 00:00:10.680

| Category: |  | TSO

| Message Details:
| Inputs:
| SIB:
| sIB7: (SysInfoType7)
| modeSpecificInfo:
| fdd:
ul_Interference: | -100
| prach_Information_SIB5_List: (DynamicPersistenceLevelList)
DynamicPersistenceLevel: | 2
| prach_Information_SIB6_List: (DynamicPersistenceLevelList)
DynamicPersistenceLevel: | 2
expirationTimeFactor: | Omit
| nonCriticalExtensions: Omit
| Outputs:
BITSTRING: |
[0] | 10 | 00 | 00 | 10 | 10 | 00 | 00 | 00
[8] | 10 | 00 | 00 | 01 |  |  |  |

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:10.680

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 18
bcch_ModificationTime: | Omit

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:10.690

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:10.690

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
| completeSIB_List:
| CompleteSIBshort:
sib_Type: | systemInformationBlockType7
sib_Data_variable: | 100000101000000010000001
| CompleteSIBshort:
sib_Type: | systemInformationBlockType18
sib_Data_variable: | 100000

#### o_SIB_PER_Encoding

RRC |  | RRC | @ 00:00:10.690

| Category: |  | TSO

| Message Details:
| Inputs:
| SIB:
| sB1: (SysInfoTypeSB1)
| sib_ReferenceList:
| SchedulingInformationSIB:
| sib_Type: (SIB_TypeAndTag)
sysInfoType6 (CellValueTag): | 2
| scheduling: (SchedulingInformation)
| scheduling:
segCount: | Omit
| sib_Pos:
rep64: | 3
| sib_PosOffsetInfo: (SibOFF_List) Omit
| SchedulingInformationSIB:
| sib_Type: (SIB_TypeAndTag)
sysInfoType7: |
| scheduling: (SchedulingInformation)
| scheduling:
segCount: | Omit
| sib_Pos:
rep16: | 2
| sib_PosOffsetInfo: (SibOFF_List) Omit
| SchedulingInformationSIB:
| sib_Type: (SIB_TypeAndTag)
sysInfoType11 (CellValueTag): | 2
| scheduling: (SchedulingInformation)
| scheduling:
segCount: | 2
| sib_Pos:
rep64: | 29
| sib_PosOffsetInfo: (SibOFF_List)
SibOFF: | so2
| SchedulingInformationSIB:
| sib_Type: (SIB_TypeAndTag)
sysInfoType12 (CellValueTag): | 2
| scheduling: (SchedulingInformation)
| scheduling:
segCount: | Omit
| sib_Pos:
rep64: | 13
| sib_PosOffsetInfo: (SibOFF_List) Omit
| SchedulingInformationSIB:
| sib_Type: (SIB_TypeAndTag)
sysInfoType18 (CellValueTag): | 2
| scheduling: (SchedulingInformation)
| scheduling:
segCount: | Omit
| sib_Pos:
rep64: | 18
| sib_PosOffsetInfo: (SibOFF_List) Omit
| nonCriticalExtensions: Omit
| Outputs:
BITSTRING: |
[0] | 00 | 01 | 00 | 00 | 10 | 10 | 10 | 00
[8] | 10 | 00 | 00 | 11 | 00 | 11 | 00 | 00
[16] | 01 | 00 | 10 | 01 | 01 | 00 | 11 | 10
[24] | 00 | 10 | 10 | 01 | 11 | 01 | 00 | 00
[32] | 00 | 00 | 01 | 01 | 10 | 10 | 00 | 10
[40] | 00 | 11 | 01 | 11 | 00 | 10 | 10 | 00
[48] | 10 | 01 | 00 | 10 |  |  |  |

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:10.690

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 4
sg_POS: | 1
bcch_ModificationTime: | Omit

#### PHY_DATA_REQ

MAC |  | PHY | @ 00:00:10.690

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCH
| CFN: |  | 54

| Message Details:
SIB repetition period: | 64
SIB position: | 20
SIB size: | 246
SIB (raw): |
[0] | 00 | 0E | 27 | 17 | 82 | 80 | 81 | 1B
[8] | 7A | 00 | 00 | 00 | 05 | B8 | C0 | 00
[16] | 80 | 12 | 10 | 23 | FF | FF | F8 | 86
[24] | 42 | 99 | 0A | 00 | 30 | 11 | 14 | 00
| SIB (decoded):
| TB 0:
MAC SDU (246 bits): |
[0] | 00 | 0E | 27 | 17 | 82 | 80 | 81 | 1B
[8] | 7A | 00 | 00 | 00 | 05 | B8 | C0 | 00
[16] | 80 | 12 | 10 | 23 | FF | FF | F8 | 86
[24] | 42 | 99 | 0A | 00 | 30 | 11 | 14 |

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:10.710

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:10.710

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
| completeSIB_List:
| CompleteSIBshort:
sib_Type: | schedulingBlock1
sib_Data_variable: | 00010000101010001000001100110000010010010100111000101001110100000000010110100010001101110010100010010010

#### o_SIB_PER_Encoding

RRC |  | RRC | @ 00:00:10.710

| Category: |  | TSO

| Message Details:
| Inputs:
| SIB:
| mIB: (MasterInformationBlock)
mib_ValueTag: | 1
| plmn_Type:
| gsm_MAP:
| plmn_Identity:
| mcc:
Digit: | 0
Digit: | 0
Digit: | 1
| mnc:
Digit: | 0
Digit: | 1
| sibSb_ReferenceList:
| SchedulingInformationSIBSb:
| sibSb_Type: (SIBSb_TypeAndTag)
sysInfoTypeSB1 (CellValueTag): | 2
| scheduling: (SchedulingInformation)
| scheduling:
segCount: | Omit
| sib_Pos:
rep16:
| 1
| sib_PosOffsetInfo: (SibOFF_List) Omit
| SchedulingInformationSIBSb:
| sibSb_Type: (SIBSb_TypeAndTag)
sysInfoType1 (PLMN_ValueTag): | 2
| scheduling: (SchedulingInformation)
| scheduling:
segCount: | Omit
| sib_Pos:
rep64: | 11
| sib_PosOffsetInfo: (SibOFF_List) Omit
| SchedulingInformationSIBSb:
| sibSb_Type: (SIBSb_TypeAndTag)
sysInfoType2 (CellValueTag): | 2
| scheduling: (SchedulingInformation)
| scheduling:
segCount: | Omit
| sib_Pos:
rep64: | 11
| sib_PosOffsetInfo: (SibOFF_List) Omit
| SchedulingInformationSIBSb:
| sibSb_Type: (SIBSb_TypeAndTag)
sysInfoType3 (CellValueTag): | 2
| scheduling: (SchedulingInformation)
| scheduling:
segCount: | Omit
| sib_Pos:
rep64: | 10
| sib_PosOffsetInfo: (SibOFF_List) Omit
| SchedulingInformationSIBSb:
| sibSb_Type: (SIBSb_TypeAndTag)
sysInfoType4 (CellValueTag): | 2
| scheduling: (SchedulingInformation)
| scheduling:
segCount: | Omit
| sib_Pos:
rep64: | 26
| sib_PosOffsetInfo: (SibOFF_List) Omit
| SchedulingInformationSIBSb:
| sibSb_Type: (SIBSb_TypeAndTag)
sysInfoType5 (CellValueTag): | 2
| scheduling: (SchedulingInformation)
| scheduling:
segCount: | 3
| sib_Pos:
rep64: | 19
| sib_PosOffsetInfo: (SibOFF_List)
SibOFF: | so4
SibOFF: | so2
| nonCriticalExtensions: Omit

| Outputs:
BITSTRING: |
[0] | 00 | 00 | 00 | 00 | 00 | 00 | 00 | 00
[8] | 01 | 00 | 00 | 00 | 00 | 10 | 01 | 01
[16] | 10 | 10 | 10 | 10 | 00 | 01 | 00 | 01
[24] | 00 | 00 | 00 | 00 | 00 | 00 | 10 | 00
[32] | 10 | 00 | 10 | 11 | 00 | 00 | 10 | 10
[40] | 00 | 10 | 00 | 10 | 11 | 00 | 01 | 00
[48] | 10 | 00 | 10 | 00 | 10 | 10 | 00 | 01
[56] | 10 | 10 | 00 | 10 | 01 | 10 | 10 | 00
[64] | 10 | 00 | 11 | 10 | 01 | 00 | 10 | 01
[72] | 00 | 11 | 00 | 01 | 00 | 01 | 00 | 00

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:10.710

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 3
sg_POS: | 0
bcch_ModificationTime: | Omit

#### PHY_DATA_REQ

MAC |  | PHY | @ 00:00:10.710

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCH
| CFN: |  | 56

| Message Details:
SIB repetition period: | 64
SIB position: | 36
SIB size: | 246
SIB (raw): |
[0] | 00 | 0E | 27 | 17 | 82 | 80 | 81 | D0
[8] | 2C | 00 | 00 | 00 | 05 | B8 | C0 | 00
[16] | 80 | 12 | 10 | 23 | FF | FF | F8 | 86
[24] | 42 | 99 | 0A | 00 | 30 | 11 | 14 | 00
| SIB (decoded):
| TB 0:
MAC SDU (246 bits): |
[0] | 00 | 0E | 27 | 17 | 82 | 80 | 81 | D0
[8] | 2C | 00 | 00 | 00 | 05 | B8 | C0 | 00
[16] | 80 | 12 | 10 | 23 | FF | FF | F8 | 86
[24] | 42 | 99 | 0A | 00 | 30 | 11 | 14 |

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:10.720

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:10.720

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
| completeSIB_List:
| CompleteSIBshort:
sib_Type: | masterInformationBlock
sib_Data_variable: | 0000000000000000010000000010010110101010000100010000000000001000100010110000101000100010110001001000100010100001101000100110100010001110010010010011000100010000

#### MMI_CmdReq

RRC |  | LLA | @ 00:00:10.720

| Message Details:
| MMI_CmdReq:
cmd (IA5String): | Please switch on the UE

#### PHY_DATA_REQ

MAC |  | PHY | @ 00:00:10.730

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCH
| CFN: |  | 58

| Message Details:
SIB repetition period: | 64
SIB position: | 52
SIB size: | 246
SIB (raw): |
[0] | 00 | 0E | 27 | 17 | 82 | 80 | 81 | 22
[8] | F0 | 00 | 00 | 00 | 0B | 71 | 80 | 01
[16] | 00 | 24 | 00 | 47 | 70 | FF | F8 | 86
[24] | 42 | 99 | 0A | 00 | 30 | 11 | 14 | 00
| SIB (decoded):
| TB 0:
MAC SDU (246 bits): |
[0] | 00 | 0E | 27 | 17 | 82 | 80 | 81 | 22
[8] | F0 | 00 | 00 | 00 | 0B | 71 | 80 | 01
[16] | 00 | 24 | 00 | 47 | 70 | FF | F8 | 86
[24] | 42 | 99 | 0A | 00 | 30 | 11 | 14 |

#### PHY_DATA_REQ

MAC |  | PHY | @ 00:00:10.750

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCH
| CFN: |  | 60

| Message Details:
SIB repetition period: | 64
SIB position: | 62
SIB size: | 246
SIB (raw): |
[0] | 00 | 00 | 27 | 17 | 82 | 80 | 81 | 22
[8] | F0 | 00 | 00 | 00 | 0B | 71 | 80 | 01
[16] | 00 | 24 | 00 | 47 | 70 | FF | F8 | 86
[24] | 42 | 99 | 0A | 00 | 30 | 11 | 14 | 00
| SIB (decoded):
| TB 0:
MAC SDU (246 bits): |
[0] | 00 | 00 | 27 | 17 | 82 | 80 | 81 | 22
[8] | F0 | 00 | 00 | 00 | 0B | 71 | 80 | 01
[16] | 00 | 24 | 00 | 47 | 70 | FF | F8 | 86
[24] | 42 | 99 | 0A | 00 | 30 | 11 | 14 |

#### PHY_DATA_REQ

MAC |  | PHY | @ 00:00:10.770

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCH
| CFN: |  | 62

| Message Details:
SIB repetition period: | 64
SIB position: | 58
SIB size: | 246
SIB (raw): |
[0] | 00 | 02 | B1 | 20 | D9 | 12 | 00 | 8C
[8] | 84 | 21 | 25 | A8 | 82 | 64 | 53 | 05
[16] | 90 | A7 | 0B | 85 | 08 | 88 | C9 | 54
[24] | 04 | A1 | 4A | 86 | 12 | 88 | 28 | 00
| SIB (decoded):
| TB 0:
MAC SDU (246 bits): |
[0] | 00 | 02 | B1 | 20 | D9 | 12 | 00 | 8C
[8] | 84 | 21 | 25 | A8 | 82 | 64 | 53 | 05
[16] | 90 | A7 | 0B | 85 | 08 | 88 | C9 | 54
[24] | 04 | A1 | 4A | 86 | 12 | 88 | 28 |

#### PHY_DATA_REQ

MAC |  | PHY | @ 00:00:10.790

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCH
| CFN: |  | 64

| Message Details:
SIB repetition period: | 64
SIB position: | 60
SIB size: | 246
SIB (raw): |
[0] | 00 | 06 | B0 | 8F | 10 | C2 | 52 | 6A
[8] | 86 | 12 | A2 | C6 | 54 | AA | 13 | E8
[16] | 88 | 14 | B0 | 8A | 15 | 78 | C9 | 54
[24] | 04 | A1 | 4A | 86 | 12 | 88 | 28 | 00
| SIB (decoded):
| TB 0:
MAC SDU (246 bits): |
[0] | 00 | 06 | B0 | 8F | 10 | C2 | 52 | 6A
[8] | 86 | 12 | A2 | C6 | 54 | AA | 13 | E8
[16] | 88 | 14 | B0 | 8A | 15 | 78 | C9 | 54
[24] | 04 | A1 | 4A | 86 | 12 | 88 | 28 |

#### PHY_DATA_REQ

MAC |  | PHY | @ 00:00:10.810

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCH
| CFN: |  | 66

| Message Details:
SIB repetition period: | 64
SIB position: | 26
SIB size: | 246
SIB (raw): |
[0] | 00 | 0E | 0C | 08 | 00 | 00 | 52 | 6A
[8] | 86 | 12 | A2 | C6 | 54 | AA | 13 | E8
[16] | 88 | 14 | B0 | 8A | 15 | 78 | C9 | 54
[24] | 04 | A1 | 4A | 86 | 12 | 88 | 28 | 00
| SIB (decoded):
| TB 0:
MAC SDU (246 bits): |
[0] | 00 | 0E | 0C | 08 | 00 | 00 | 52 | 6A
[8] | 86 | 12 | A2 | C6 | 54 | AA | 13 | E8
[16] | 88 | 14 | B0 | 8A | 15 | 78 | C9 | 54
[24] | 04 | A1 | 4A | 86 | 12 | 88 | 28 |

#### PHY_DATA_REQ

MAC |  | PHY | @ 00:00:10.830

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCH
| CFN: |  | 68

| Message Details:
SIB repetition period: | 64
SIB position: | 28
SIB size: | 246
SIB (raw): |
[0] | 00 | 00 | 0C | 08 | 00 | 00 | 52 | 6A
[8] | 86 | 12 | A2 | C6 | 54 | AA | 13 | E8
[16] | 88 | 14 | B0 | 8A | 15 | 78 | C9 | 54
[24] | 04 | A1 | 4A | 86 | 12 | 88 | 28 | 00
| SIB (decoded):
| TB 0:
MAC SDU (246 bits): |
[0] | 00 | 00 | 0C | 08 | 00 | 00 | 52 | 6A
[8] | 86 | 12 | A2 | C6 | 54 | AA | 13 | E8
[16] | 88 | 14 | B0 | 8A | 15 | 78 | C9 | 54
[24] | 04 | A1 | 4A | 86 | 12 | 88 | 28 |

#### PHY_DATA_REQ

MAC |  | PHY | @ 00:00:10.850

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCH
| CFN: |  | 70

| Message Details:
SIB repetition period: | 64
SIB position: | 30
SIB size: | 246
SIB (raw): |
[0] | 00 | 00 | 0C | 08 | 00 | 00 | 52 | 6A
[8] | 86 | 12 | A2 | C6 | 54 | AA | 13 | E8
[16] | 88 | 14 | B0 | 8A | 15 | 78 | C9 | 54
[24] | 04 | A1 | 4A | 86 | 12 | 88 | 28 | 00
| SIB (decoded):
| TB 0:
MAC SDU (246 bits): |
[0] | 00 | 00 | 0C | 08 | 00 | 00 | 52 | 6A
[8] | 86 | 12 | A2 | C6 | 54 | AA | 13 | E8
[16] | 88 | 14 | B0 | 8A | 15 | 78 | C9 | 54
[24] | 04 | A1 | 4A | 86 | 12 | 88 | 28 |

#### PHY_DATA_REQ

MAC |  | PHY | @ 00:00:10.870

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCH
| CFN: |  | 72

| Message Details:
SIB repetition period: | 64
SIB position: | 36
SIB size: | 246
SIB (raw): |
[0] | 00 | 0E | 27 | 17 | 82 | 80 | 81 | D0
[8] | 2C | 00 | A2 | C6 | 54 | AA | 13 | E8
[16] | 88 | 14 | B0 | 8A | 15 | 78 | C9 | 54
[24] | 04 | A1 | 4A | 86 | 12 | 88 | 28 | 00
| SIB (decoded):
| TB 0:
MAC SDU (246 bits): |
[0] | 00 | 0E | 27 | 17 | 82 | 80 | 81 | D0
[8] | 2C | 00 | A2 | C6 | 54 | AA | 13 | E8
[16] | 88 | 14 | B0 | 8A | 15 | 78 | C9 | 54
[24] | 04 | A1 | 4A | 86 | 12 | 88 | 28 |

#### PHY_DATA_REQ

MAC |  | PHY | @ 00:00:10.890

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCH
| CFN: |  | 74

| Message Details:
SIB repetition period: | 16
SIB position: | 2
SIB size: | 246
SIB (raw): |
[0] | 00 | 0E | 1B | 67 | 10 | A8 | 83 | 30
[8] | 49 | 4E | 29 | D0 | 05 | A2 | 37 | 28
[16] | 92 | 14 | B0 | 8A | 15 | 78 | C9 | 54
[24] | 04 | A1 | 4A | 86 | 12 | 88 | 28 | 00
| SIB (decoded):
| TB 0:
MAC SDU (246 bits): |
[0] | 00 | 0E | 1B | 67 | 10 | A8 | 83 | 30
[8] | 49 | 4E | 29 | D0 | 05 | A2 | 37 | 28
[16] | 92 | 14 | B0 | 8A | 15 | 78 | C9 | 54
[24] | 04 | A1 | 4A | 86 | 12 | 88 | 28 |

#### PHY_DATA_REQ

MAC |  | PHY | @ 00:00:10.910

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCH
| CFN: |  | 76

| Message Details:
SIB repetition period: | 8
SIB position: | 0
SIB size: | 246
SIB (raw): |
[0] | 00 | 0E | 00 | 9F | 00 | 00 | 40 | 25
[8] | AA | 11 | 00 | 08 | 8B | 0A | 22 | C4
[16] | 88 | A1 | A2 | 68 | 8E | 49 | 31 | 10
[24] | 04 | A1 | 4A | 86 | 12 | 88 | 28 | 00
| SIB (decoded):
| TB 0:
MAC SDU (246 bits): |
[0]
| 00 | 0E | 00 | 9F | 00 | 00 | 40 | 25
[8] | AA | 11 | 00 | 08 | 8B | 0A | 22 | C4
[16] | 88 | A1 | A2 | 68 | 8E | 49 | 31 | 10
[24] | 04 | A1 | 4A | 86 | 12 | 88 | 28 |

#### MMI_CmdCnf

LLA |  | RRC | @ 00:00:11.970

| Message Details:
| MMI_CmdCnf:
result: | true
resultString (IA5String): | Omit

#### PHY_DATA_IND

PHY |  | MAC | @ 00:00:20.790

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: U_RACH
| CFN: |  | 20

| Message Details:
TFI: | 0
TB set size: | 168
TB size: | 168
TB set (raw): |
[0] | 08 | 44 | 48 | 8C | D1 | 00 | 04 | 02
[8] | 00 | 02 | C0 | 00 | 00 | 00 | 00 | 00
[16] | 00 | 00 | 00 | 00 | 00 | 00 |  |
| TB set (decoded):
| TB 0:
TCTF: | 0
MAC SDU (166 bits): |
[0] | 21 | 11 | 22 | 33 | 44 | 00 | 10 | 08
[8] | 00 | 0B | 00 | 00 | 00 | 00 | 00 | 00
[16] | 00 | 00 | 00 | 00 | 00 |  |  |

#### RLC_TR_DATA_IND

LLA |  | RRC | @ 00:00:20.800

| Channel ID: |  | Rb0
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_IND:
cellId: | 0
| routingInfo:
rB_Identity:
| 0
| tM_message:
| uL_CCCH_Message:
| integrityCheckInfo: Omit
| message: (UL_CCCH_MessageType)
| rrcConnectionRequest:
| initialUE_Identity:
| tmsi_and_LAI: (TMSI_and_LAI_GSM_MAP)
tmsi (TMSI_GSM_MAP):
| 00010001001000100011001101000100
| lai:
| plmn_Identity:
| mcc:
Digit:
| 0
Digit: | 0
Digit: | 1
| mnc:
Digit: | 0
Digit: | 1

lac: | 0000000000000001

establishmentCause: | registration
protocolErrorIndicator: | noError

| measuredResultsOnRACH: Omit

| v3d0NonCriticalExtensions: Omit

#### RLC_UM_DATA_REQ

RRC |  | LLA | @ 00:00:20.820

| Channel ID: |  | Rb0
| Cell ID: |  | 0

| Message Details:
| RLC_UM_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | 0
| uM_message:
| dL_CCCH_Message:
| integrityCheckInfo: Omit
| message: (DL_CCCH_MessageType)
| rrcConnectionSetup:
| r3:
| rrcConnectionSetup_r3: (RRCConnectionSetup_r3_IEs)
| initialUE_Identity:
| tmsi_and_LAI: (TMSI_and_LAI_GSM_MAP)
tmsi (TMSI_GSM_MAP): | 00010001001000100011001101000100
| lai:
| plmn_Identity:
| mcc:
Digit: | 0
Digit: | 0
Digit: | 1
| mnc:
Digit: | 0
Digit: | 1

lac: | 0000000000000001

rrc_TransactionIdentifier: | 0
activationTime: | Omit

| new_U_RNTI: (U_RNTI)
srnc_Identity: | 000000000001
s_RNTI: | 00000000000000000001

new_c_RNTI (C_RNTI): | Omit
rrc_StateIndicator: | cell_DCH
utran_DRX_CycleLengthCoeff (UTRAN_DRX_CycleLengthCoefficient): | 9

| capabilityUpdateRequirement:
ue_RadioCapabilityFDDUpdateRequirement: | true
ue_RadioCapabilityTDDUpdateRequirement: | false
| systemSpecificCapUpdateReqList:
SystemSpecificCapUpdateReq: | gsm

| srb_InformationSetupList: (SRB_InformationSetupList2)
| SRB_InformationSetup:
rb_Identity: | Omit
| rlc_InfoChoice:
| rlc_Info:
| ul_RLC_Mode:
| ul_UM_RLC_Mode:
| transmissionRLC_Discard: Omit

| dl_RLC_Mode:
dl_UM_RLC_Mode: |

| rb_MappingInfo:
| RB_MappingOption:
| ul_LogicalChannelMappings:
| oneLogicalChannel: (UL_LogicalChannelMapping)
| ul_TransportChannelType:
dch (TransportChannelIdentity): | 5
logicalChannelIdentity: | 1
| rlc_SizeList:
configured: |
mac_LogicalChannelPriority: | 1

| dl_LogicalChannelMappingList:
| DL_LogicalChannelMapping:
| dl_TransportChannelType:
dch (TransportChannelIdentity): | 10
logicalChannelIdentity: | 1

| RB_MappingOption:
| ul_LogicalChannelMappings:
| oneLogicalChannel: (UL_LogicalChannelMapping)
| ul_TransportChannelType:
rach: |
logicalChannelIdentity: | 1
| rlc_SizeList:
| explicitList: (RLC_SizeExplicitList)
| RLC_SizeInfo:
rlc_SizeIndex: | 1

mac_LogicalChannelPriority: | 1

| dl_LogicalChannelMappingList:
| DL_LogicalChannelMapping:
| dl_TransportChannelType:
fach: |
logicalChannelIdentity: | 1

| SRB_InformationSetup:
rb_Identity: | Omit
| rlc_InfoChoice:
| rlc_Info:
| ul_RLC_Mode:
| ul_AM_RLC_Mode:
| transmissionRLC_Discard:
noDiscard (MaxDAT): | dat15
transmissionWindowSize: | tw32
timerRST: | tr500
max_RST (MaxRST): | rst1
| pollingInfo:
timerPollProhibit: | tpp200
timerPoll: | tp200
poll_PDU: | Omit
poll_SDU: | sdu1
lastTransmissionPDU_Poll: | true
lastRetransmissionPDU_Poll: | true
pollWindow: | pw99
timerPollPeriodic: | Omit

| dl_RLC_Mode:
| dl_AM_RLC_Mode:
inSequenceDelivery: | true
receivingWindowSize: | rw32
| dl_RLC_StatusInfo:
timerStatusProhibit: | tsp200
timerEPC: | Omit
missingPDU_Indicator: | true
timerStatusPeriodic: | Omit

| rb_MappingInfo:
| RB_MappingOption:
| ul_LogicalChannelMappings:
| oneLogicalChannel: (UL_LogicalChannelMapping)
| ul_TransportChannelType:
dch (TransportChannelIdentity): | 5
logicalChannelIdentity: | 2
| rlc_SizeList:
configured: |
mac_LogicalChannelPriority: | 2

| dl_LogicalChannelMappingList:
| DL_LogicalChannelMapping:
| dl_TransportChannelType:
dch (TransportChannelIdentity): | 10
logicalChannelIdentity: | 2

| RB_MappingOption:
| ul_LogicalChannelMappings:
| oneLogicalChannel: (UL_LogicalChannelMapping)
| ul_TransportChannelType:
rach: |
logicalChannelIdentity: | 2
| rlc_SizeList:
| explicitList: (RLC_SizeExplicitList)
| RLC_SizeInfo:
rlc_SizeIndex: | 1

mac_LogicalChannelPriority: | 2

| dl_LogicalChannelMappingList:
| DL_LogicalChannelMapping:
| dl_TransportChannelType:
fach: |
logicalChannelIdentity: | 2

| SRB_InformationSetup:
rb_Identity: | Omit
| rlc_InfoChoice:
| rlc_Info:
| ul_RLC_Mode:
| ul_AM_RLC_Mode:
| transmissionRLC_Discard:
noDiscard (MaxDAT): | dat15
transmissionWindowSize: | tw32
timerRST: | tr500
max_RST (MaxRST): | rst1
| pollingInfo:
timerPollProhibit: | tpp200
timerPoll: | tp200
poll_PDU: | Omit
poll_SDU: | sdu1
lastTransmissionPDU_Poll: | true
lastRetransmissionPDU_Poll: | true
pollWindow: | pw99
timerPollPeriodic: | Omit

| dl_RLC_Mode:
| dl_AM_RLC_Mode:
inSequenceDelivery: | true
receivingWindowSize: | rw32
| dl_RLC_StatusInfo:
timerStatusProhibit: | tsp200
timerEPC: | Omit
missingPDU_Indicator: | true
timerStatusPeriodic: | Omit

| rb_MappingInfo:
| RB_MappingOption:
| ul_LogicalChannelMappings:
| oneLogicalChannel: (UL_LogicalChannelMapping)
| ul_TransportChannelType:
dch (TransportChannelIdentity): | 5
logicalChannelIdentity: | 3
| rlc_SizeList:
configured: |
mac_LogicalChannelPriority: | 3

| dl_LogicalChannelMappingList:
| DL_LogicalChannelMapping:
| dl_TransportChannelType:
dch (TransportChannelIdentity): | 10
logicalChannelIdentity: | 3

| RB_MappingOption:
| ul_LogicalChannelMappings:
| oneLogicalChannel: (UL_LogicalChannelMapping)
| ul_TransportChannelType:
rach: |
logicalChannelIdentity: | 3
| rlc_SizeList:
| explicitList: (RLC_SizeExplicitList)
| RLC_SizeInfo:
rlc_SizeIndex: | 1

mac_LogicalChannelPriority: | 3

| dl_LogicalChannelMappingList:
| DL_LogicalChannelMapping:
| dl_TransportChannelType:
fach: |
logicalChannelIdentity: | 3

| SRB_InformationSetup:
rb_Identity: | Omit
| rlc_InfoChoice:
| rlc_Info:
| ul_RLC_Mode:
| ul_AM_RLC_Mode:
| transmissionRLC_Discard:
noDiscard (MaxDAT): | dat15
transmissionWindowSize: | tw32
timerRST: | tr500
max_RST (MaxRST): | rst1
| pollingInfo:
timerPollProhibit: | tpp200
timerPoll: | tp200
poll_PDU: | Omit
poll_SDU: | sdu1
lastTransmissionPDU_Poll: | true
lastRetransmissionPDU_Poll: | true
pollWindow: | pw99
timerPollPeriodic: | Omit

| dl_RLC_Mode:
| dl_AM_RLC_Mode:
inSequenceDelivery: | true
receivingWindowSize: | rw32
| dl_RLC_StatusInfo:
timerStatusProhibit: | tsp200
timerEPC: | Omit
missingPDU_Indicator: | true
timerStatusPeriodic: | Omit

| rb_MappingInfo:
| RB_MappingOption:
| ul_LogicalChannelMappings:
| oneLogicalChannel: (UL_LogicalChannelMapping)
| ul_TransportChannelType:
dch (TransportChannelIdentity): | 5
logicalChannelIdentity: | 4
| rlc_SizeList:
configured: |
mac_LogicalChannelPriority: | 4

| dl_LogicalChannelMappingList:
| DL_LogicalChannelMapping:
| dl_TransportChannelType:
dch (TransportChannelIdentity): | 10
logicalChannelIdentity: | 4

| RB_MappingOption:
| ul_LogicalChannelMappings:
| oneLogicalChannel: (UL_LogicalChannelMapping)
| ul_TransportChannelType:
rach: |
logicalChannelIdentity: | 4
| rlc_SizeList:
| explicitList: (RLC_SizeExplicitList)
| RLC_SizeInfo:
rlc_SizeIndex: | 1

mac_LogicalChannelPriority: | 4

| dl_LogicalChannelMappingList:
| DL_LogicalChannelMapping:
| dl_TransportChannelType:
fach: |
logicalChannelIdentity: | 4

| ul_CommonTransChInfo:
| tfc_Subset: Omit
| prach_TFCS: (TFCS) Omit
| modeSpecificInfo:
| fdd:
| ul_TFCS: (TFCS)
| normalTFCI_Signalling: (ExplicitTFCS_Configuration)
| complete: (TFCS_ReconfAdd)
| ctfcSize:
| ctfc2Bit:
| :
ctfc2: | 0
| powerOffsetInformation:
| gainFactorInformation:
computedGainFactors (ReferenceTFC_ID): | 0
powerOffsetPp_m: | Omit

| :
ctfc2: | 1
| powerOffsetInformation:
| gainFactorInformation:
| signalledGainFactors:
| modeSpecificInfo:
| fdd:
gainFactorBetaC (GainFactor): | 11

gainFactorBetaD (GainFactor): | 15
referenceTFC_ID: | 0

powerOffsetPp_m: | Omit

| ul_AddReconfTransChInfoList:
| UL_AddReconfTransChInformation:
ul_TransportChannelType (UL_TrCH_Type): | dch
transportChannelIdentity: | 5
| transportFormatSet:
| dedicatedTransChTFS:
| tti:
| tti10: (DedicatedDynamicTF_InfoList)
| DedicatedDynamicTF_Info:
| rlc_Size:
| bitMode: (BitModeRLC_SizeInfo)
| sizeType2:
part1: | 2
part2: | Omit

| numberOfTbSizeList:
| NumberOfTransportBlocks:
zero: |
| NumberOfTransportBlocks:
one: |

| logicalChannelList:
allSizes: |

| semistaticTF_Information:
| channelCodingType:
convolutional (CodingRate): | third
rateMatchingAttribute: | 192
crc_Size: | crc16

| dl_CommonTransChInfo:
| sccpch_TFCS: (TFCS) Omit
| modeSpecificInfo:
| fdd:
| dl_Parameters:
sameAsUL: |

| dl_AddReconfTransChInfoList:
| DL_AddReconfTransChInformation:
dl_TransportChannelType (DL_TrCH_Type): | dch
dl_transportChannelIdentity (TransportChannelIdentity): | 10
| tfs_SignallingMode:
| sameAsULTrCH: (UL_TransportChannelIdentity)
ul_TransportChannelType (UL_TrCH_Type): | dch
ul_TransportChannelIdentity (TransportChannelIdentity): | 5

| dch_QualityTarget: (QualityTarget)
bler_QualityValue: | -20

| dummy: (TM_SignallingInfo) Omit

| frequencyInfo: Omit

maxAllowedUL_TX_Power: | Omit

| ul_ChannelRequirement:
| ul_DPCH_Info:
| ul_DPCH_PowerControlInfo:
| fdd:
dpcch_PowerOffset: | -40
pc_Preamble: | 1
sRB_delay: | 7
| powerControlAlgorithm:
algorithm1 (TPC_StepSizeFDD): | 0

| modeSpecificInfo:
| fdd:
scramblingCodeType: | longSC
scramblingCode (UL_ScramblingCode): | 0
numberOfDPDCH: | Omit
spreadingFactor: | sf64
tfci_Existence: | true
numberOfFBI_Bits: | Omit
puncturingLimit: | pl1

| dl_CommonInformation:
| dl_DPCH_InfoCommon:
| cfnHandling:
| initialise:
cfntargetsfnframeoffset: | Omit

| modeSpecificInfo:
| fdd:
| dl_DPCH_PowerControlInfo:
| modeSpecificInfo:
| fdd:
dpc_Mode: | singleTPC

powerOffsetPilot_pdpdch: | 0

| dl_rate_matching_restriction: Omit

| spreadingFactorAndPilot: (SF512_AndPilot)
sfd128 (PilotBits128): | pb4

positionFixedOrFlexible: | fixed
tfci_Existence: | false

| modeSpecificInfo:
| fdd:
defaultDPCH_OffsetValue (DefaultDPCH_OffsetValueFDD): | 0
| dpch_CompressedModeInfo: Omit
tx_DiversityMode: | noDiversity
| ssdt_Information: Omit

| dl_InformationPerRL_List:
| DL_InformationPerRL:
| modeSpecificInfo:
| fdd:
| primaryCPICH_Info:
primaryScramblingCode: | 100
| pdsch_SHO_DCH_Info: Omit
| pdsch_CodeMapping: Omit

| dl_DPCH_InfoPerRL:
| fdd:
pCPICH_UsageForChannelEst: | mayBeUsed
dpch_FrameOffset: | 0
| secondaryCPICH_Info: Omit
| dl_ChannelisationCodeList:
| DL_ChannelisationCode:
secondaryScramblingCode: | 1
| sf_AndCodeNumber: (SF512_AndCodeNumber)
sf128: | 0
scramblingCodeChange: | noCodeChange

tpc_CombinationIndex: | 0
ssdt_CellIdentity: | Omit
closedLoopTimingAdjMode: | Omit

| sccpch_InfoforFACH: Omit

| laterNonCriticalExtensions: Omit

specialLI: | true

#### CMAC Configuration REQ

LLA |  | MAC | @ 00:00:20.850

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: S_CCPCH
| CFN: |  | 46

| Message Details:
| Configuration Parameters:
Number Of Transport Channels: | 3
| Transport Channels:
| Item Number 0:
| Transport Channel Parameters:
| Transport Channel:
Name: | PCH
Identity: | 0
TTI (ms): | 10
EP Type: | 1/2 Rate Convolutional Coding
CRC Size: | 16
RM Attribute: | 230
First Interleave: | On
Number Of Transport Formats: | 2
| Transport Format Set:
| Transport Format 0:
Number Of Transport Blocks: | 0
Transport Block Size In Bits: | 240
| Transport Format 1:
Number Of Transport Blocks: | 1
Transport Block Size In Bits: | 240

Number Of Logical Channels: | 1

| Logical Channels:
| Item Number 0:
| Logical Channel:
Name:
| PCCH
Identity: | 0

Priority: | 1
CT Length: | 0
CT Value: | 0
TCTF Length: | 0
TCTF Value: | 0
UE ID Type: | Not used
UE ID: | 0

| Item Number 1:
| Transport Channel Parameters:
| Transport Channel:
Name:
| FACH
Identity: | 0

TTI (ms): | 10
EP Type: | 1/2 Rate Convolutional Coding
CRC Size: | 16
RM Attribute: | 220
First Interleave: | On
Number Of Transport Formats: | 3

| Transport Format Set:
| Transport Format 0:
Number Of Transport Blocks:
| 0
Transport Block Size In Bits: | 168

| Transport Format 1:
Number Of Transport Blocks: | 1
Transport Block Size In Bits: | 168

| Transport Format 2:
Number Of Transport Blocks: | 2
Transport Block Size In Bits: | 168

Number Of Logical Channels: | 1

| Logical Channels:
| Item Number 0:
| Logical Channel:
Name:
| CCCH
Identity: | 1

Priority: | 1
CT Length: | 0
CT Value: | 0
TCTF Length: | 8
TCTF Value: | 64
UE ID Type: | Not used
UE ID: | 0

| Item Number 2:
| Transport Channel Parameters:
| Transport Channel:
Name:
| FACH
Identity: | 1

TTI (ms): | 10
EP Type: | Turbo Coding
CRC Size: | 16
RM Attribute: | 130
First Interleave: | On
Number Of Transport Formats: | 2

| Transport Format Set:
| Transport Format 0:
Number Of Transport Blocks:
| 0
Transport Block Size In Bits: | 360

| Transport Format 1:
Number Of Transport Blocks: | 1
Transport Block Size In Bits: | 360

Number Of Logical Channels: | 0

Active Flag: | 1

| Transport Format Combination Set:
Number Of Transport Format Combinations: | 8
| Transport Format Combinations 0:
Transport Format:
| 0
Transport Format: | 0
Transport Format: | 0

| Transport Format Combinations 1:
Transport Format: | 1
Transport Format: | 0
Transport Format: | 0

| Transport Format Combinations 2:
Transport Format: | 0
Transport Format: | 1
Transport Format: | 0

| Transport Format Combinations 3:
Transport Format: | 1
Transport Format: | 1
Transport Format: | 0

| Transport Format Combinations 4:
Transport Format: | 0
Transport Format: | 2
Transport Format: | 0

| Transport Format Combinations 5:
Transport Format: | 1
Transport Format: | 2
Transport Format: | 0

| Transport Format Combinations 6:
Transport Format: | 0
Transport Format: | 0
Transport Format: | 1

| Transport Format Combinations 7:
Transport Format: | 0
Transport Format: | 1
Transport Format: | 1

#### CMAC Configuration CNF

MAC |  | LLA | @ 00:00:20.850

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: S_CCPCH
| CFN: |  | 46

| Message Details:

#### PHY_DATA_REQ

MAC |  | PHY | @ 00:00:20.880

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: FACH
| CFN: |  | 49

| Message Details:
TFI: | 2
TB set size: | 336
TB size: | 168
TB set (raw, each TB word aligned): |
[0] | 40 | 01 | F8 | 30 | E7 | 22 | 24 | 46
[8] | 68 | 80 | 02 | 01 | 00 | 01 | 00 | 04
[16] | 00 | 00 | 4D | 82 | 69 | 00 | 40 | 02
[24] | 3A | 10 | 10 | 89 | 0D | 42 | 00 | 02
[32] | 81 | 9E | 8E | 46 | C9 | A6 | 7C | 9C
[40] | 4E | 74 | 20 | 00 |  |  |  |

| TB set (decoded):
| TB 0:
TCTF: | 64
MAC SDU (160 bits): |
[0] | 01 | F8 | 30 | E7 | 22 | 24 | 46 | 68
[8] | 80 | 02 | 01 | 00 | 01 | 00 | 04 | 00
[16] | 00 | 4D | 82 | 69 |  |  |  |

| TB 1:
TCTF: | 64
MAC SDU (160 bits): |
[0] | 02 | 3A | 10 | 10 | 89 | 0D | 42 | 00
[8] | 02 | 81 | 9E | 8E | 46 | C9 | A6 | 7C
[16] | 9C | 4E | 74 | 20 |  |  |  |

#### PHY_DATA_REQ

MAC |  | PHY | @ 00:00:20.890

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: FACH
| CFN: |  | 50

| Message Details:
TFI: | 2
TB set size: | 336
TB size: | 168
TB set (raw, each TB word aligned): |
[0] | 40 | 04 | A5 | 12 | 3A | 8C | 00 | 15
[8] | 13 | 3D | 1C | 8D | 93 | 4C | F9 | 38
[16] | 9C | E8 | 42 | 52 | 24 | 00 | 40 | 06
[24] | B5 | 28 | 00 | 4A | 46 | 7A | 39 | 1B
[32] | 26 | 99 | F2 | 71 | 39 | D0 | 86 | B4
[40] | 49 | EA | 70 | 00 |  |  |  |

| TB set (decoded):
| TB 0:
TCTF: | 64
MAC SDU (160 bits): |
[0] | 04 | A5 | 12 | 3A | 8C | 00 | 15 | 13
[8] | 3D | 1C | 8D | 93 | 4C | F9 | 38 | 9C
[16] | E8 | 42 | 52 | 24 |  |  |  |

| TB 1:
TCTF:
| 64
MAC SDU (160 bits): |
[0]
| 06 | B5 | 28 | 00 | 4A | 46 | 7A | 39
[8] | 1B | 26 | 99 | F2 | 71 | 39 | D0 | 86
[16] | B4 | 49 | EA | 70 |  |  |  |

#### PHY_DATA_REQ

MAC |  | PHY | @ 00:00:20.900

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: FACH
| CFN: |  | 51

| Message Details:
TFI:
| 2
TB set size: | 336
TB size: | 168
TB set (raw, each TB word aligned): |
[0]
| 40 | 08 | 00 | D4 | C8 | 00 | 06 | 25
[8] | 2B | F0 | 02 | 00 | 08 | 82 | 23 | BF
[16] | 66 | 08 | 98 | 95 | A5 | 00 | 40 | 0B
[24] | 23 | FE | 47 | 82 | 00 | 00 | 01 | 3F
[32] | 90 | 0A | 14 | 00 | 02 | 06 | 40 | 00
[40] | 0C | 28 | 08 | 00 |  |  |  |

| TB set (decoded):
| TB 0:
TCTF: | 64
MAC SDU (160 bits): |
[0] | 08 | 00 | D4 | C8 | 00 | 06 | 25 | 2B
[8] | F0 | 02 | 00 | 08 | 82 | 23 | BF | 66
[16] | 08 | 98 | 95 | A5 |  |  |  |

| TB 1:
TCTF: | 64
MAC SDU (160 bits): |
[0] | 0B | 23 | FE | 47 | 82 | 00 | 00 | 01
[8] | 3F | 90 | 0A | 14 | 00 | 02 | 06 | 40
[16] | 00 | 0C | 28 | 08 |  |  |  |

#### CPHY_SYNC_IND

PHY |  | RRC | @ 00:00:21.130

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: U_DPCH
| CFN: |  | 74

| Message Details:

#### PHY_DATA_IND

PHY |  | MAC | @ 00:00:21.320

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: U_DCH
| CFN: |  | 73

| Message Details:
TFI: | 1
TB set size: | 148
TB size: | 148
TB set (raw): |
[0] | 18 | 00 | 04 | A0 | 80 | 00 | 5A | 00
[8] | 05 | 99 | 1A | 85 | 50 | 6A | 4C | 26
[16] | 84 | 62 | C0 | 00 |  |  |  |

| TB set (decoded):
| TB 0:
C/T: | 1
MAC SDU (144 bits): |
[0] | 80 | 00 | 4A | 08 | 00 | 05 | A0 | 00
[8] | 59 | 91 | A8 | 55 | 06 | A4 | C2 | 68
[16] | 46 | 2C |  |  |  |  |  |

#### PHY_DATA_IND

PHY |  | MAC | @ 00:00:21.330

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: U_DCH
| CFN: |  | 74

| Message Details:
TFI: | 1
TB set size: | 148
TB size: | 148
TB set (raw): |
[0] | 18 | 00 | D1 | 5F | E9 | 40 | 20 | 80
[8] | 00 | 80 | 01 | 18 | A1 | 40 | 00 | 00
[16] | 00 | 00 | 00 | 00 |  |  |  |

| TB set (decoded):
| TB 0:
C/T: | 1
MAC SDU (144 bits): |
[0] | 80 | 0D | 15 | FE | 94 | 02 | 08 | 00
[8] | 08 | 00 | 11 | 8A | 14 | 00 | 00 | 00
[16] | 00 | 00 |  |  |  |  |  |

#### PHY_DATA_REQ

MAC |  | PHY | @ 00:00:21.340

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: DCH
| CFN: |  | 95

| Message Details: | TFI: | 1 TB set size: | 148 TB size: | 148 TB set (raw): | [0] | 10 | 20 | 02 | 00 | 00 | 00 | 00 | 00 [8] | 00 | 00 | 00 | 00 | 00 | 00 | 00 | 00 [16] | 00 | 00 | 00 | 00 |  |  |  |

| TB set (decoded):
| TB 0:
C/T: | 1
MAC SDU (144 bits): |
[0] | 02 | 00 | 20 | 00 | 00 | 00 | 00 | 00
[8] | 00 | 00 | 00 | 00 | 00 | 00 | 00 | 00
[16] | 00 | 00 |  |  |  |  |  |

#### RLC_AM_DATA_IND

LLA |  | RRC | @ 00:00:21.360

| Channel ID: |  | Rb2 | Cell ID: |  | -1

| Message Details: |  | RLC_AM_DATA_IND: | cellId: | -1

| routingInfo: | rB_Identity: | 2

integrityResult:

integrityUsed (IntegrityStatus):i_pass

aM_message:

uL_DCCH_Message:

integrityCheckInfo: Omit

message: (UL_DCCH_MessageType)

rrcConnectionSetupComplete:

rrc_TransactionIdentifier:0

| startList: |  | STARTSingle: | cn_DomainIdentity: | cs_domain start_Value: | 00000000000000010110

STARTSingle:

cn_DomainIdentity:ps_domain
start_Value:00000000000000101100

ue_RadioAccessCapability:

accessStratumReleaseIndicator:r99

| pdcp_Capability: | losslessSRNS_RelocationSupport: | true

| supportForRfc2507: | notSupported: |

rlc_Capability:

totalRLC_AM_BufferSize:kb50
maximumRLC_WindowSize:mws2047
maximumAM_EntityNumber (MaximumAM_EntityNumberRLC_Cap):am6

transportChannelCapability:

dl_TransChCapability:

maxNoBitsReceived (MaxNoBits):b6400
maxConvCodeBitsReceived (MaxNoBits):b640

| turboDecodingSupport: (TurboSupport) | supported (MaxNoBits): | b6400

maxSimultaneousTransChs (MaxSimultaneousTransChsDL):e8
maxSimultaneousCCTrCH_Count:1
maxReceivedTransportBlocks (MaxTransportBlocksDL):tb32
maxNumberOfTFC (MaxNumberOfTFC_DL):tfc128
maxNumberOfTF:tf64

ul_TransChCapability:

maxNoBitsTransmitted (MaxNoBits):b3840
maxConvCodeBitsTransmitted (MaxNoBits):b640

| turboEncodingSupport: (TurboSupport) | supported (MaxNoBits): | b3840

maxSimultaneousTransChs (MaxSimultaneousTransChsUL):e8

| modeSpecificInfo: | fdd: |

maxTransmittedBlocks (MaxTransportBlocksUL):tb8
maxNumberOfTFC (MaxNumberOfTFC_UL):tfc32
maxNumberOfTF:tf32

rf_Capability:

fddRF_Capability:

ue_PowerClass:4
txRxFrequencySeparation:mhz190

tddRF_Capability: Omit

physicalChannelCapability:

fddPhysChCapability:

downlinkPhysChCapability: (DL_PhysChCapabilityFDD)

maxNoDPCH_PDSCH_Codes:3
maxNoPhysChBitsReceived:b19200
supportForSF_512:false
supportOfPDSCH:false

| simultaneousSCCPCH_DPCH_Reception: | notSupported: |

uplinkPhysChCapability: (UL_PhysChCapabilityFDD)

maxNoDPDCH_BitsTransmitted:b2400
supportOfPCPCH:false

tddPhysChCapability: Omit

ue_MultiModeRAT_Capability:

multiRAT_CapabilityList: (MultiRAT_Capability)

supportOfGSM:false
supportOfMulticarrier:false

multiModeCapability:fdd

securityCapability:

cipheringAlgorithmCap:0000000000000001
integrityProtectionAlgorithmCap:0000000000000010

ue_positioning_Capability:

standaloneLocMethodsSupported:false
ue_BasedOTDOA_Supported:false
networkAssistedGPS_Supported:noNetworkAssistedGPS
supportForUE_GPS_TimingOfCellFrames:false
supportForIPDL:false

measurementCapability:

downlinkCompressedMode: (CompressedModeMeasCapability)

fdd_Measurements:true
tdd_Measurements: Omit

| gsm_Measurements: | gsm900: | false dcs1800: | false gsm1900: | false

multiCarrierMeasurements: Omit

uplinkCompressedMode: (CompressedModeMeasCapability)

fdd_Measurements:true
tdd_Measurements: Omit

| gsm_Measurements: | gsm900: | false dcs1800: | false gsm1900: | false

multiCarrierMeasurements: Omit

ue_RATSpecificCapability: (InterRAT_UE_RadioAccessCapabilityList) Omit

v370NonCriticalExtensions: Omit

#### PHY_DATA_IND

PHY MAC @ 00:00:21.550

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 96

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 00 D1 5F E9 40 20 80
[8]00 80 01 18 A1 40 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 0D 15 FE 94 02 08 00
[8]08 00 11 8A 14 00 00 00
[16]00 00

#### PHY_DATA_REQ

MAC PHY @ 00:00:21.560

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 117

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]10 20 02 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]02 00 20 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:00:21.580

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 99

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 00 01 58 0D 10 0E 84
[8]00 81 62 80 01 86 01 82
[16]FA 09 10 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 00 15 80 D1 00 E8 40
[8]08 16 28 00 18 60 18 2F
[16]A0 91

#### PHY_DATA_IND

PHY MAC @ 00:00:21.590

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 100

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 00 8A 2B 3C 00 78 88
[8]00 00 82 82 A1 67 00 02
[16]00 0C D0 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 08 A2 B3 C0 07 88 80
[8]00 08 28 2A 16 70 00 20
[16]00 CD

#### PHY_DATA_IND

PHY MAC @ 00:00:21.600

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 101

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 01 50 DF E5 89 1A 20
[8]00 58 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 15 0D FE 58 91 A2 00
[8]05 80 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_REQ

MAC PHY @ 00:00:21.610

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 122

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 03 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_REQ

MAC PHY @ 00:00:21.650

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 126

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 00 01 42 04 E1 02 40
[8]26 04 2A AA AA AA AA AA
[16]AA AA A0 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 00 14 20 4E 10 24 02
[8]60 42 AA AA AA AA AA AA
[16]AA AA

#### PHY_DATA_REQ

MAC PHY @ 00:00:21.660

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 127

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 00 8A AA AA AA AA AA
[8]AA AA B0 05 02 0C C2 20
[16]06 64 50 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 08 AA AA AA AA AA AA
[8]AA AB 00 50 20 CC 22 00
[16]66 45

#### PHY_DATA_REQ

MAC PHY @ 00:00:21.670

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 128

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 01 51 7F EB A0 00 0A
[8]A8 8E EC C2 20 06 64 40
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 15 17 FE BA 00 00 AA
[8]88 EE CC 22 00 66 44 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:00:21.820

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 123

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 01 50 DF E5 89 1A 20
[8]00 58 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 15 0D FE 58 91 A2 00
[8]05 80 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_REQ

MAC PHY @ 00:00:21.830

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 144

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 03 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_REQ

MAC PHY @ 00:00:21.850

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 146

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 01 51 7F EB A0 00 0A
[8]A8 8E EC C2 20 06 64 40
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 15 17 FE BA 00 00 AA
[8]88 EE CC 22 00 66 44 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:00:21.910

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 132

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 03 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:00:22.130

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 154

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 03 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:00:22.140

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 155

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 01 86 C8 06 84 09 81
[8]91 2A A2 3B B3 14 82 08
[16]80 19 90 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 18 6C 80 68 40 98 19
[8]12 AA 23 BB 31 48 20 88
[16]01 99

#### PHY_DATA_IND

PHY MAC @ 00:00:22.150

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 156

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 02 50 3F E1 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 25 03 FE 10 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### CRLC_SecurityMode_Config_REQ

RRC LLA @ 00:00:22.160

Cell ID: -1

Message Details:

CRLC_SecurityMode_Config_REQ:

cellId:-1

rlcSecurityInfo: (SecurityInfo)

cn_DomainIdentity:ps_domain
startValue (START_Value):00000000000000000000
cipheringKey: Omit
integrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
gsmCipheringKey: Omit

#### PHY_DATA_REQ

MAC PHY @ 00:00:22.160

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 177

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 05 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 50 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### CRLC_SecurityMode_Config_CNF

LLA RRC @ 00:00:22.180

Cell ID: -1

Message Details:

CRLC_SecurityMode_Config_CNF:

cellId:-1

#### CRLC_SetRRC_MessageSN_REQ

RRC LLA @ 00:00:22.180

Channel ID: Rb0
Cell ID: 0

Message Details:

CRLC_SetRRC_MessageSN_REQ:

cellId:0

routingInfo:

rB_Identity:0

count_I_LSB_UL (RRC_SequenceNumber): Omit
count_I_LSB_DL (RRC_SequenceNumber):0

#### CRLC_SetRRC_MessageSN_CNF

LLA RRC @ 00:00:22.190

Channel ID: Rb0
Cell ID: 0

Message Details:

CRLC_SetRRC_MessageSN_CNF:

cellId:0

routingInfo:

rB_Identity:0

#### CRLC_SetRRC_MessageSN_REQ

RRC LLA @ 00:00:22.190

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_REQ:

cellId:-1

routingInfo:

rB_Identity:1

count_I_LSB_UL (RRC_SequenceNumber): Omit
count_I_LSB_DL (RRC_SequenceNumber):0

#### CRLC_SetRRC_MessageSN_CNF

LLA RRC @ 00:00:22.210

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_CNF:

cellId:-1

routingInfo:

rB_Identity:1

#### CRLC_SetRRC_MessageSN_REQ

RRC LLA @ 00:00:22.210

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_REQ:

cellId:-1

routingInfo:

rB_Identity:2

count_I_LSB_UL (RRC_SequenceNumber): Omit
count_I_LSB_DL (RRC_SequenceNumber):0

#### CRLC_SetRRC_MessageSN_CNF

LLA RRC @ 00:00:22.220

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_CNF:

cellId:-1

routingInfo:

rB_Identity:2

#### CRLC_SetRRC_MessageSN_REQ

RRC LLA @ 00:00:22.220

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_REQ:

cellId:-1

routingInfo:

rB_Identity:3

count_I_LSB_UL (RRC_SequenceNumber): Omit
count_I_LSB_DL (RRC_SequenceNumber):0

#### CRLC_SetRRC_MessageSN_CNF

LLA RRC @ 00:00:22.240

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_CNF:

cellId:-1

routingInfo:

rB_Identity:3

#### CRLC_SetRRC_MessageSN_REQ

RRC LLA @ 00:00:22.240

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_REQ:

cellId:-1

routingInfo:

rB_Identity:4

count_I_LSB_UL (RRC_SequenceNumber): Omit
count_I_LSB_DL (RRC_SequenceNumber):0

#### CRLC_SetRRC_MessageSN_CNF

LLA RRC @ 00:00:22.250

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_CNF:

cellId:-1

routingInfo:

rB_Identity:4

#### CRLC_Integrity_Activate_REQ

RRC LLA @ 00:00:22.250

Cell ID: -1

Message Details:

CRLC_Integrity_Activate_REQ:

cellId:-1
cn_DomainIdentity:ps_domain

integrityActivationInfo:

integrityProtectionModeInfo:

integrityProtectionModeCommand:

startIntegrityProtection:

integrityProtInitNumber:00001111000011110000111100001111

integrityProtectionAlgorithm:uia1

#### CRLC_Integrity_Activate_CNF

LLA RRC @ 00:00:22.270

Cell ID: -1

Message Details:

CRLC_Integrity_Activate_CNF:

cellId:-1

#### CRLC_Integrity_Activate_REQ

RRC LLA @ 00:00:22.270

Cell ID: -1

Message Details:

CRLC_Integrity_Activate_REQ:

cellId:-1
cn_DomainIdentity:ps_domain

integrityActivationInfo:

ul_IntegProtActivationInfo: (IntegrityProtActivationInfoList)

SS_IntegrityProtActivationTimeInfo:

rb_Identity:2
rrc_MessageSequenceNumber:0

#### CMAC Integrity Check Request

RRC MAC @ 00:00:22.290

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000001
Data:

[0]00 00 00 01
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:1 (RNC to UE)
Message Length (bits):128
Message:

[0]80 00 00 01 04 06 00 00
[8]80 01 41 E1 E1 E1 F0 00

#### CMAC Integrity Check Result

MAC RRC @ 00:00:22.290

Message Details:

Integrity Check Result:

MAC-I:11101000011101111000001101000000
Data:

[0]E8 77 83 40

#### CRLC_Integrity_Activate_CNF

LLA RRC @ 00:00:22.290

Cell ID: -1

Message Details:

CRLC_Integrity_Activate_CNF:

cellId:-1

#### RLC_AM_DATA_REQ

RRC LLA @ 00:00:22.290

Channel ID: Rb2
Cell ID: -1

Message Details:

RLC_AM_DATA_REQ:

cellId:-1

routingInfo:

rB_Identity:2

confirmationRequest: (AmConfirmationRequest)

noConfirmationRequest:

aM_message:

dL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode:00000000000000000000000000000000
rrc_MessageSequenceNumber:0

message: (DL_DCCH_MessageType)

securityModeCommand:

r3:

securityModeCommand_r3: (SecurityModeCommand_r3_IEs)

rrc_TransactionIdentifier:0

securityCapability:

cipheringAlgorithmCap:0000000000000001
integrityProtectionAlgorithmCap:0000000000000010

cipheringModeInfo: Omit

integrityProtectionModeInfo:

integrityProtectionModeCommand:

startIntegrityProtection:

integrityProtInitNumber:00001111000011110000111100001111

integrityProtectionAlgorithm:uia1

cn_DomainIdentity:ps_domain

ue_SystemSpecificSecurityCap: (InterRAT_UE_SecurityCapList)

InterRAT_UE_SecurityCapability:

gsm:

gsmSecurityCapability:0000000

laterNonCriticalExtensions: Omit

#### PHY_DATA_REQ

MAC PHY @ 00:00:22.300

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 191

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 00 0F 43 BC 1A 00 C0
[8]60 00 08 00 14 1E 1E 1E
[16]1F 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 00 F4 3B C1 A0 0C 06
[8]00 00 80 01 41 E1 E1 E1
[16]F0 00

#### PHY_DATA_REQ

MAC PHY @ 00:00:22.310

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 192

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 00 D0 1F E0 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 0D 01 FE 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:00:22.370

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 178

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 02 50 3F E1 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 25 03 FE 10 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_REQ

MAC PHY @ 00:00:22.380

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 199

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 05 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 50 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_REQ

MAC PHY @ 00:00:22.500

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 211

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 00 D0 1F E0 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 0D 01 FE 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:00:22.550

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 196

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]10 20 02 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]02 00 20 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:00:22.560

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 197

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 01 51 3F EC 59 1B E7
[8]10 D2 10 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 15 13 FE C5 91 BE 71
[8]0D 21 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_REQ

MAC PHY @ 00:00:22.570

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 218

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]10 20 03 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### CMAC Integrity Check Request

RRC MAC @ 00:00:22.580

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000001
Data:

[0]00 00 00 01
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:0 (UE to RNC)
Message Length (bits):72
Message:

[0]80 00 00 01 05 21 00 00
[8]00

#### CMAC Integrity Check Result

MAC RRC @ 00:00:22.580

Message Details:

Integrity Check Result:

MAC-I:10001011001000110111110011100010
Data:

[0]8B 23 7C E2

#### RLC_AM_DATA_IND

LLA RRC @ 00:00:22.580

Channel ID: Rb2
Cell ID: -1

Message Details:

RLC_AM_DATA_IND:

cellId:-1

routingInfo:

rB_Identity:2

integrityResult:

integrityUsed (IntegrityStatus):i_pass

aM_message:

uL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode:10001011001000110111110011100010
rrc_MessageSequenceNumber:1

message: (UL_DCCH_MessageType)

securityModeComplete:

rrc_TransactionIdentifier:0

ul_IntegProtActivationInfo: (IntegrityProtActivationInfo)

rrc_MessageSequenceNumberList:

RRC_MessageSequenceNumber:0
RRC_MessageSequenceNumber:0
RRC_MessageSequenceNumber:0
RRC_MessageSequenceNumber:0
RRC_MessageSequenceNumber:0

rb_UL_CiphActivationTimeInfo: (RB_ActivationTimeInfoList) Omit

laterNonCriticalExtensions: Omit

#### CRLC_Integrity_Activate_REQ

RRC LLA @ 00:00:22.580

Cell ID: -1

Message Details:

CRLC_Integrity_Activate_REQ:

cellId:-1
cn_DomainIdentity:ps_domain

integrityActivationInfo:

ul_IntegProtActivationInfo: (IntegrityProtActivationInfoList)

SS_IntegrityProtActivationTimeInfo:

rb_Identity:0
rrc_MessageSequenceNumber:0

SS_IntegrityProtActivationTimeInfo:

rb_Identity:1
rrc_MessageSequenceNumber:0

SS_IntegrityProtActivationTimeInfo:

rb_Identity:3
rrc_MessageSequenceNumber:0

SS_IntegrityProtActivationTimeInfo:

rb_Identity:4
rrc_MessageSequenceNumber:0

#### CMAC Integrity Check Request

RRC MAC @ 00:00:22.600

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000001
Data:

[0]00 00 00 01
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:1 (RNC to UE)
Message Length (bits):296
Message:

[0]80 00 00 01 81 42 03 81
[8]00 40 7C 00 80 1E 22 00
[16]00 20 A3 35 62 46 83 00
[24]BE 82 46 8A CF 04 60 BE
[32]82 24 46 68 80

#### CMAC Integrity Check Result

MAC RRC @ 00:00:22.600

Message Details:

Integrity Check Result:

MAC-I:10100000000110000010111001100001
Data:

[0]A0 18 2E 61

#### CRLC_Integrity_Activate_CNF

LLA RRC @ 00:00:22.600

Cell ID: -1

Message Details:

CRLC_Integrity_Activate_CNF:

cellId:-1

#### PHY_DATA_REQ

MAC PHY @ 00:00:22.610

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 222

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 01 8D 00 C1 73 08 94
[8]20 38 10 04 07 C0 08 01
[16]E2 20 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 18 D0 0C 17 30 89 42
[8]03 81 00 40 7C 00 80 1E
[16]22 00

#### PHY_DATA_REQ

MAC PHY @ 00:00:22.620

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 223

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 02 00 02 0A 33 56 24
[8]68 30 0B E8 24 68 AC F0
[16]46 0B E0 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 20 00 20 A3 35 62 46
[8]83 00 BE 82 46 8A CF 04
[16]60 BE

#### PHY_DATA_REQ

MAC PHY @ 00:00:22.630

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 224

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 02 D0 BF E8 22 44 66
[8]88 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 2D 0B FE 82 24 46 68
[8]80 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:00:22.770

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 218

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]10 20 02 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]02 00 20 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:00:22.780

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 219

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 01 51 3F EC 59 1B E7
[8]10 D2 10 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 15 13 FE C5 91 BE 71
[8]0D 21 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_REQ

MAC PHY @ 00:00:22.790

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 240

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]10 20 03 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_REQ

MAC PHY @ 00:00:22.810

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 242

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 02 D0 BF E8 22 44 66
[8]88 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 2D 0B FE 82 24 46 68
[8]80 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:00:22.870

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 228

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 06 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 60 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:00:22.880

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 229

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 02 D1 5F ED 6F 6F 71
[8]E0 EC 80 08 40 18 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 2D 15 FE D6 F6 F7 1E
[8]0E C8 00 84 01 80 00 00
[16]00 00

#### PHY_DATA_REQ

MAC PHY @ 00:00:22.890

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 250

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 06 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 60 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### CMAC Integrity Check Request

RRC MAC @ 00:00:22.890

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000001
Data:

[0]00 00 00 01
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:0 (UE to RNC)
Message Length (bits):80
Message:

[0]80 00 00 01 86 C8 00 84
[8]01 80

#### CMAC Integrity Check Result

MAC RRC @ 00:00:22.890

Message Details:

Integrity Check Result:

MAC-I:10101101111011011110111000111100
Data:

[0]AD ED EE 3C

#### PHY_DATA_IND

PHY MAC @ 00:00:23.090

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 250

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 06 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 60 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:00:23.100

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 251

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 02 D1 5F ED 6F 6F 71
[8]E0 EC 80 08 40 18 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 2D 15 FE D6 F6 F7 1E
[8]0E C8 00 84 01 80 00 00
[16]00 00

#### PHY_DATA_REQ

MAC PHY @ 00:00:23.110

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 16

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 06 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 60 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### CMAC Integrity Check Request

RRC MAC @ 00:00:23.910

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000001
Data:

[0]00 00 00 01
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:1 (RNC to UE)
Message Length (bits):56
Message:

[0]80 00 00 00 83 C8 00

#### CMAC Integrity Check Result

MAC RRC @ 00:00:23.910

Message Details:

Integrity Check Result:

MAC-I:11101100100111000001011111010011
Data:

[0]EC 9C 17 D3

#### RLC_UM_DATA_REQ

RRC LLA @ 00:00:23.910

Channel ID: Rb1
Cell ID: -1

Message Details:

RLC_UM_DATA_REQ:

cellId:-1

routingInfo:

rB_Identity:1

uM_message:

dL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode:00000000000000000000000000000000
rrc_MessageSequenceNumber:0

message: (DL_DCCH_MessageType)

rrcConnectionRelease:

r3:

rrcConnectionRelease_r3: (RRCConnectionRelease_r3_IEs)

rrc_TransactionIdentifier:0
n_308:1
releaseCause:normalEvent

rplmn_information: Omit

laterNonCriticalExtensions: Omit

specialLI:false

#### PHY_DATA_REQ

MAC PHY @ 00:00:23.920

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 97

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]00 10 FF EF 64 E0 BE 98
[8]BC 80 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:0
MAC SDU (144 bits):

[0]01 0F FE F6 4E 0B E9 8B
[8]C8 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:00:24.160

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 101

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]00 10 DF EF BF 16 16 70
[8]C4 00 B0 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:0
MAC SDU (144 bits):

[0]01 0D FE FB F1 61 67 0C
[8]40 0B 00 00 00 00 00 00
[16]00 00

#### CMAC Integrity Check Request

RRC MAC @ 00:00:24.180

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000001
Data:

[0]00 00 00 01
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:0 (UE to RNC)
Message Length (bits):48
Message:

[0]80 00 00 00 84 40

#### CMAC Integrity Check Result

MAC RRC @ 00:00:24.180

Message Details:

Integrity Check Result:

MAC-I:11110111111000101100001011001110
Data:

[0]F7 E2 C2 CE

#### RLC_UM_DATA_IND

LLA RRC @ 00:00:24.180

Channel ID: Rb1
Cell ID: -1

Message Details:

RLC_UM_DATA_IND:

cellId:-1

routingInfo:

rB_Identity:1

integrityResult:

integrityUsed (IntegrityStatus):i_pass

uM_message:

uL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode:11110111111000101100001011001110
rrc_MessageSequenceNumber:1

message: (UL_DCCH_MessageType)

rrcConnectionReleaseComplete:

rrc_TransactionIdentifier:0

errorIndication: (FailureCauseWithProtErr) Omit

laterNonCriticalExtensions: Omit

#### PHY_DATA_IND

PHY MAC @ 00:00:24.320

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 117

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]00 30 DF ED CD 18 3E 01
[8]44 00 B0 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:0
MAC SDU (144 bits):

[0]03 0D FE DC D1 83 E0 14
[8]40 0B 00 00 00 00 00 00
[16]00 00

#### CMAC Integrity Check Request

RRC MAC @ 00:00:24.350

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000010
Data:

[0]00 00 00 02
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:0 (UE to RNC)
Message Length (bits):48
Message:

[0]80 00 00 00 84 40

#### CMAC Integrity Check Result

MAC RRC @ 00:00:24.350

Message Details:

Integrity Check Result:

MAC-I:10111001101000110000011111000000
Data:

[0]B9 A3 07 C0

#### RLC_UM_DATA_IND

LLA RRC @ 00:00:24.350

Channel ID: Rb1
Cell ID: -1

Message Details:

RLC_UM_DATA_IND:

cellId:-1

routingInfo:

rB_Identity:1

integrityResult:

integrityUsed (IntegrityStatus):i_pass

uM_message:

uL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode:10111001101000110000011111000000
rrc_MessageSequenceNumber:2

message: (UL_DCCH_MessageType)

rrcConnectionReleaseComplete:

rrc_TransactionIdentifier:0

errorIndication: (FailureCauseWithProtErr) Omit

laterNonCriticalExtensions: Omit

#### CRLC_Config_REQ

RRC LLA @ 00:00:24.350

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:1

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC_Config_CNF

LLA RRC @ 00:00:24.360

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:1

#### CRLC_Config_REQ

RRC LLA @ 00:00:24.360

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:2

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CPHY_OUTSYNC_IND

PHY RRC @ 00:00:24.380

BTS unit: 1:1
Channel No: 0 Name: U_DPCH
CFN: 143

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:00:24.380

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:2

#### CRLC_Config_REQ

RRC LLA @ 00:00:24.380

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:3

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC_Config_CNF

LLA RRC @ 00:00:24.390

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:3

#### CRLC_Config_REQ

RRC LLA @ 00:00:24.390

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:4

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC_Config_CNF

LLA RRC @ 00:00:24.410

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:4

#### CRLC_Config_REQ

RRC LLA @ 00:00:24.410

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:1

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode)

dl_UM_RLC_Mode:

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):136

dl_RLCModeInfo: (UL_RLC_Mode)

ul_UM_RLC_Mode:

transmissionRLC_Discard:

timerBasedNoExplicit (NoExplicitDiscard):dt100

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity):1
dLlogicalChannelIdentity (LogicalChannelIdentity):1
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC_Config_CNF

LLA RRC @ 00:00:24.430

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:1

#### CRLC_Config_REQ

RRC LLA @ 00:00:24.430

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:2

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode)

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):128

dl_RLCModeInfo: (UL_RLC_Mode)

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity):2
dLlogicalChannelIdentity (LogicalChannelIdentity):2
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC_Config_CNF

LLA RRC @ 00:00:24.440

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:2

#### CRLC_Config_REQ

RRC LLA @ 00:00:24.440

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:3

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode)

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):128

dl_RLCModeInfo: (UL_RLC_Mode)

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity):3
dLlogicalChannelIdentity (LogicalChannelIdentity):3
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC_Config_CNF

LLA RRC @ 00:00:24.460

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:3

#### CRLC_Config_REQ

RRC LLA @ 00:00:24.460

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:4

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode)

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):128

dl_RLCModeInfo: (UL_RLC_Mode)

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity):4
dLlogicalChannelIdentity (LogicalChannelIdentity):4
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC_Config_CNF

LLA RRC @ 00:00:24.470

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:4

#### MMI_CmdReq

RRC LLA @ 00:00:29.490

Message Details:

MMI_CmdReq:

cmd (IA5String):Please switch off the UE

#### MMI_CmdCnf

LLA RRC @ 00:00:31.110

Message Details:

MMI_CmdCnf:

result:true
resultString (IA5String): Omit

#### PHY_DATA_IND

PHY MAC @ 00:00:34.170

BTS unit: 1:1
Channel No: 0 Name: U_RACH
CFN: 78

Message Details:

TFI:0
TB set size:168
TB size:168
TB set (raw):

[0]08 44 48 8C D1 00 04 02
[8]00 02 D0 00 00 00 00 00
[16]00 00 00 00 00 00

TB set (decoded):

TB 0:

TCTF:0
MAC SDU (166 bits):

[0]21 11 22 33 44 00 10 08
[8]00 0B 40 00 00 00 00 00
[16]00 00 00 00 00

#### RLC_TR_DATA_IND

LLA RRC @ 00:00:34.190

Channel ID: Rb0
Cell ID: 0

Message Details:

RLC_TR_DATA_IND:

cellId:0

routingInfo:

rB_Identity:0

tM_message:

uL_CCCH_Message:

integrityCheckInfo: Omit

message: (UL_CCCH_MessageType)

rrcConnectionRequest:

initialUE_Identity:

tmsi_and_LAI: (TMSI_and_LAI_GSM_MAP)

tmsi (TMSI_GSM_MAP):00010001001000100011001101000100

lai:

plmn_Identity:

mcc:

Digit:0
Digit:0
Digit:1

mnc:

Digit:0
Digit:1

lac:0000000000000001

establishmentCause:detach
protocolErrorIndicator:noError

measuredResultsOnRACH: Omit

v3d0NonCriticalExtensions: Omit

#### RLC_UM_DATA_REQ

RRC LLA @ 00:00:34.190

Channel ID: Rb0
Cell ID: 0

Message Details:

RLC_UM_DATA_REQ:

cellId:0

routingInfo:

rB_Identity:0

uM_message:

dL_CCCH_Message:

integrityCheckInfo: Omit

message: (DL_CCCH_MessageType)

rrcConnectionSetup:

r3:

rrcConnectionSetup_r3: (RRCConnectionSetup_r3_IEs)

initialUE_Identity:

tmsi_and_LAI: (TMSI_and_LAI_GSM_MAP)

tmsi (TMSI_GSM_MAP):00010001001000100011001101000100

lai:

plmn_Identity:

mcc:

Digit:0
Digit:0
Digit:1

mnc:

Digit:0
Digit:1

lac:0000000000000001

rrc_TransactionIdentifier:0
activationTime: Omit

new_U_RNTI: (U_RNTI)

srnc_Identity:000000000001
s_RNTI:00000000000000000001

new_c_RNTI (C_RNTI): Omit
rrc_StateIndicator:cell_DCH
utran_DRX_CycleLengthCoeff (UTRAN_DRX_CycleLengthCoefficient):9

capabilityUpdateRequirement:

ue_RadioCapabilityFDDUpdateRequirement:true
ue_RadioCapabilityTDDUpdateRequirement:false

systemSpecificCapUpdateReqList:

SystemSpecificCapUpdateReq:gsm

srb_InformationSetupList: (SRB_InformationSetupList2)

SRB_InformationSetup:

rb_Identity: Omit

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_UM_RLC_Mode:

transmissionRLC_Discard: Omit

dl_RLC_Mode:

dl_UM_RLC_Mode:

rb_MappingInfo:

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

dch (TransportChannelIdentity):5

logicalChannelIdentity:1

rlc_SizeList:

configured:

mac_LogicalChannelPriority:1

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

dch (TransportChannelIdentity):10

logicalChannelIdentity:1

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

rach:

logicalChannelIdentity:1

rlc_SizeList:

explicitList: (RLC_SizeExplicitList)

RLC_SizeInfo:

rlc_SizeIndex:1

mac_LogicalChannelPriority:1

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

fach:

logicalChannelIdentity:1

SRB_InformationSetup:

rb_Identity: Omit

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

rb_MappingInfo:

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

dch (TransportChannelIdentity):5

logicalChannelIdentity:2

rlc_SizeList:

configured:

mac_LogicalChannelPriority:2

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

dch (TransportChannelIdentity):10

logicalChannelIdentity:2

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

rach:

logicalChannelIdentity:2

rlc_SizeList:

explicitList: (RLC_SizeExplicitList)

RLC_SizeInfo:

rlc_SizeIndex:1

mac_LogicalChannelPriority:2

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

fach:

logicalChannelIdentity:2

SRB_InformationSetup:

rb_Identity: Omit

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

rb_MappingInfo:

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

dch (TransportChannelIdentity):5

logicalChannelIdentity:3

rlc_SizeList:

configured:

mac_LogicalChannelPriority:3

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

dch (TransportChannelIdentity):10

logicalChannelIdentity:3

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

rach:

logicalChannelIdentity:3

rlc_SizeList:

explicitList: (RLC_SizeExplicitList)

RLC_SizeInfo:

rlc_SizeIndex:1

mac_LogicalChannelPriority:3

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

fach:

logicalChannelIdentity:3

SRB_InformationSetup:

rb_Identity: Omit

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

rb_MappingInfo:

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

dch (TransportChannelIdentity):5

logicalChannelIdentity:4

rlc_SizeList:

configured:

mac_LogicalChannelPriority:4

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

dch (TransportChannelIdentity):10

logicalChannelIdentity:4

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

rach:

logicalChannelIdentity:4

rlc_SizeList:

explicitList: (RLC_SizeExplicitList)

RLC_SizeInfo:

rlc_SizeIndex:1

mac_LogicalChannelPriority:4

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

fach:

logicalChannelIdentity:4

ul_CommonTransChInfo:

tfc_Subset: Omit

prach_TFCS: (TFCS) Omit

modeSpecificInfo:

fdd:

ul_TFCS: (TFCS)

normalTFCI_Signalling: (ExplicitTFCS_Configuration)

complete: (TFCS_ReconfAdd)

ctfcSize:

ctfc2Bit:

:

ctfc2:0

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc2:1

powerOffsetInformation:

gainFactorInformation:

signalledGainFactors:

modeSpecificInfo:

fdd:

gainFactorBetaC (GainFactor):11

gainFactorBetaD (GainFactor):15
referenceTFC_ID:0

powerOffsetPp_m: Omit

ul_AddReconfTransChInfoList:

UL_AddReconfTransChInformation:

ul_TransportChannelType (UL_TrCH_Type):dch
transportChannelIdentity:5

transportFormatSet:

dedicatedTransChTFS:

tti:

tti10: (DedicatedDynamicTF_InfoList)

DedicatedDynamicTF_Info:

rlc_Size:

bitMode: (BitModeRLC_SizeInfo)

sizeType2:

part1:2
part2: Omit

numberOfTbSizeList:

NumberOfTransportBlocks:

zero:

NumberOfTransportBlocks:

one:

logicalChannelList:

allSizes:

semistaticTF_Information:

channelCodingType:

convolutional (CodingRate):third

rateMatchingAttribute:192
crc_Size:crc16

dl_CommonTransChInfo:

sccpch_TFCS: (TFCS) Omit

modeSpecificInfo:

fdd:

dl_Parameters:

sameAsUL:

dl_AddReconfTransChInfoList:

DL_AddReconfTransChInformation:

dl_TransportChannelType (DL_TrCH_Type):dch
dl_transportChannelIdentity (TransportChannelIdentity):10

tfs_SignallingMode:

sameAsULTrCH: (UL_TransportChannelIdentity)

ul_TransportChannelType (UL_TrCH_Type):dch
ul_TransportChannelIdentity (TransportChannelIdentity):5

dch_QualityTarget: (QualityTarget)

bler_QualityValue:-20

dummy: (TM_SignallingInfo) Omit

frequencyInfo: Omit

maxAllowedUL_TX_Power: Omit

ul_ChannelRequirement:

ul_DPCH_Info:

ul_DPCH_PowerControlInfo:

fdd:

dpcch_PowerOffset:-40
pc_Preamble:1
sRB_delay:7

powerControlAlgorithm:

algorithm1 (TPC_StepSizeFDD):0

modeSpecificInfo:

fdd:

scramblingCodeType:longSC
scramblingCode (UL_ScramblingCode):0
numberOfDPDCH: Omit
spreadingFactor:sf64
tfci_Existence:true
numberOfFBI_Bits: Omit
puncturingLimit:pl1

dl_CommonInformation:

dl_DPCH_InfoCommon:

cfnHandling:

initialise:

cfntargetsfnframeoffset: Omit

modeSpecificInfo:

fdd:

dl_DPCH_PowerControlInfo:

modeSpecificInfo:

fdd:

dpc_Mode:singleTPC

powerOffsetPilot_pdpdch:0

dl_rate_matching_restriction: Omit

spreadingFactorAndPilot: (SF512_AndPilot)

sfd128 (PilotBits128):pb4

positionFixedOrFlexible:fixed
tfci_Existence:false

modeSpecificInfo:

fdd:

defaultDPCH_OffsetValue (DefaultDPCH_OffsetValueFDD):0

dpch_CompressedModeInfo: Omit

tx_DiversityMode:noDiversity

ssdt_Information: Omit

dl_InformationPerRL_List:

DL_InformationPerRL:

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode:100

pdsch_SHO_DCH_Info: Omit

pdsch_CodeMapping: Omit

dl_DPCH_InfoPerRL:

fdd:

pCPICH_UsageForChannelEst:mayBeUsed
dpch_FrameOffset:0

secondaryCPICH_Info: Omit

dl_ChannelisationCodeList:

DL_ChannelisationCode:

secondaryScramblingCode:1

sf_AndCodeNumber: (SF512_AndCodeNumber)

sf128:0

scramblingCodeChange:noCodeChange

tpc_CombinationIndex:0
ssdt_CellIdentity: Omit
closedLoopTimingAdjMode: Omit

sccpch_InfoforFACH: Omit

laterNonCriticalExtensions: Omit

specialLI:true

#### PHY_DATA_REQ

MAC PHY @ 00:00:34.230

BTS unit: 1:1
Channel No: 0 Name: FACH
CFN: 104

Message Details:

TFI:2
TB set size:336
TB size:168
TB set (raw, each TB word aligned):

[0]40 0D F8 30 E7 22 24 46
[8]68 80 02 01 00 01 00 04
[16]00 00 4D 82 69 00 40 0E
[24]3A 10 10 89 0D 42 00 02
[32]81 9E 8E 46 C9 A6 7C 9C
[40]4E 74 20 00

TB set (decoded):

TB 0:

TCTF:64
MAC SDU (160 bits):

[0]0D F8 30 E7 22 24 46 68
[8]80 02 01 00 01 00 04 00
[16]00 4D 82 69

TB 1:

TCTF:64
MAC SDU (160 bits):

[0]0E 3A 10 10 89 0D 42 00
[8]02 81 9E 8E 46 C9 A6 7C
[16]9C 4E 74 20

#### PHY_DATA_REQ

MAC PHY @ 00:00:34.240

BTS unit: 1:1
Channel No: 0 Name: FACH
CFN: 105

Message Details:

TFI:2
TB set size:336
TB size:168
TB set (raw, each TB word aligned):

[0]40 10 A5 12 3A 8C 00 15
[8]13 3D 1C 8D 93 4C F9 38
[16]9C E8 42 52 24 00 40 12
[24]B5 28 00 4A 46 7A 39 1B
[32]26 99 F2 71 39 D0 86 B4
[40]49 EA 70 00

TB set (decoded):

TB 0:

TCTF:64
MAC SDU (160 bits):

[0]10 A5 12 3A 8C 00 15 13
[8]3D 1C 8D 93 4C F9 38 9C
[16]E8 42 52 24

TB 1:

TCTF:64
MAC SDU (160 bits):

[0]12 B5 28 00 4A 46 7A 39
[8]1B 26 99 F2 71 39 D0 86
[16]B4 49 EA 70

#### PHY_DATA_REQ

MAC PHY @ 00:00:34.250

BTS unit: 1:1
Channel No: 0 Name: FACH
CFN: 106

Message Details:

TFI:2
TB set size:336
TB size:168
TB set (raw, each TB word aligned):

[0]40 14 00 D4 C8 00 06 25
[8]2B F0 02 00 08 82 23 BF
[16]66 08 98 95 A5 00 40 17
[24]23 FE 47 82 00 00 01 3F
[32]90 0A 14 00 02 06 40 00
[40]0C 28 08 00

TB set (decoded):

TB 0:

TCTF:64
MAC SDU (160 bits):

[0]14 00 D4 C8 00 06 25 2B
[8]F0 02 00 08 82 23 BF 66
[16]08 98 95 A5

TB 1:

TCTF:64
MAC SDU (160 bits):

[0]17 23 FE 47 82 00 00 01
[8]3F 90 0A 14 00 02 06 40
[16]00 0C 28 08

#### CPHY_SYNC_IND

PHY RRC @ 00:00:34.510

BTS unit: 1:1
Channel No: 0 Name: U_DPCH
CFN: 132

Message Details:

#### PHY_DATA_IND

PHY MAC @ 00:00:34.690

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 130

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 00 04 A0 80 00 5A 00
[8]00 59 1A 85 50 6A 4C 26
[16]84 62 C0 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 00 4A 08 00 05 A0 00
[8]05 91 A8 55 06 A4 C2 68
[16]46 2C

#### PHY_DATA_IND

PHY MAC @ 00:00:34.700

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 131

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 00 D1 5F E9 40 20 80
[8]00 80 01 18 A1 40 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 0D 15 FE 94 02 08 00
[8]08 00 11 8A 14 00 00 00
[16]00 00

#### RLC_AM_DATA_IND

LLA RRC @ 00:00:34.710

Channel ID: Rb2
Cell ID: -1

Message Details:

RLC_AM_DATA_IND:

cellId:-1

routingInfo:

rB_Identity:2

integrityResult:

integrityUsed (IntegrityStatus):i_pass

aM_message:

uL_DCCH_Message:

integrityCheckInfo: Omit

message: (UL_DCCH_MessageType)

rrcConnectionSetupComplete:

rrc_TransactionIdentifier:0

startList:

STARTSingle:

cn_DomainIdentity:cs_domain
start_Value:00000000000000010110

STARTSingle:

cn_DomainIdentity:ps_domain
start_Value:00000000000000000010

ue_RadioAccessCapability:

accessStratumReleaseIndicator:r99

pdcp_Capability:

losslessSRNS_RelocationSupport:true

supportForRfc2507:

notSupported:

rlc_Capability:

totalRLC_AM_BufferSize:kb50
maximumRLC_WindowSize:mws2047
maximumAM_EntityNumber (MaximumAM_EntityNumberRLC_Cap):am6

transportChannelCapability:

dl_TransChCapability:

maxNoBitsReceived (MaxNoBits):b6400
maxConvCodeBitsReceived (MaxNoBits):b640

turboDecodingSupport: (TurboSupport)

supported (MaxNoBits):b6400

maxSimultaneousTransChs (MaxSimultaneousTransChsDL):e8
maxSimultaneousCCTrCH_Count:1
maxReceivedTransportBlocks (MaxTransportBlocksDL):tb32
maxNumberOfTFC (MaxNumberOfTFC_DL):tfc128
maxNumberOfTF:tf64

ul_TransChCapability:

maxNoBitsTransmitted (MaxNoBits):b3840
maxConvCodeBitsTransmitted (MaxNoBits):b640

turboEncodingSupport: (TurboSupport)

supported (MaxNoBits):b3840

maxSimultaneousTransChs (MaxSimultaneousTransChsUL):e8

modeSpecificInfo:

fdd:

maxTransmittedBlocks (MaxTransportBlocksUL):tb8
maxNumberOfTFC (MaxNumberOfTFC_UL):tfc32
maxNumberOfTF:tf32

rf_Capability:

fddRF_Capability:

ue_PowerClass:4
txRxFrequencySeparation:mhz190

tddRF_Capability: Omit

physicalChannelCapability:

fddPhysChCapability:

downlinkPhysChCapability: (DL_PhysChCapabilityFDD)

maxNoDPCH_PDSCH_Codes:3
maxNoPhysChBitsReceived:b19200
supportForSF_512:false
supportOfPDSCH:false

simultaneousSCCPCH_DPCH_Reception:

notSupported:

uplinkPhysChCapability: (UL_PhysChCapabilityFDD)

maxNoDPDCH_BitsTransmitted:b2400
supportOfPCPCH:false

tddPhysChCapability: Omit

ue_MultiModeRAT_Capability:

multiRAT_CapabilityList: (MultiRAT_Capability)

supportOfGSM:false
supportOfMulticarrier:false

multiModeCapability:fdd

securityCapability:

cipheringAlgorithmCap:0000000000000001
integrityProtectionAlgorithmCap:0000000000000010

ue_positioning_Capability:

standaloneLocMethodsSupported:false
ue_BasedOTDOA_Supported:false
networkAssistedGPS_Supported:noNetworkAssistedGPS
supportForUE_GPS_TimingOfCellFrames:false
supportForIPDL:false

measurementCapability:

downlinkCompressedMode: (CompressedModeMeasCapability)

fdd_Measurements:true
tdd_Measurements: Omit

gsm_Measurements:

gsm900:false
dcs1800:false
gsm1900:false

multiCarrierMeasurements: Omit

uplinkCompressedMode: (CompressedModeMeasCapability)

fdd_Measurements:true
tdd_Measurements: Omit

gsm_Measurements:

gsm900:false
dcs1800:false
gsm1900:false

multiCarrierMeasurements: Omit

ue_RATSpecificCapability: (InterRAT_UE_RadioAccessCapabilityList) Omit

v370NonCriticalExtensions: Omit

#### PHY_DATA_REQ

MAC PHY @ 00:00:34.710

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 152

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]10 20 02 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]02 00 20 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:00:34.920

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 153

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 00 D1 5F E9 40 20 80
[8]00 80 01 18 A1 40 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 0D 15 FE 94 02 08 00
[8]08 00 11 8A 14 00 00 00
[16]00 00

#### PHY_DATA_REQ

MAC PHY @ 00:00:34.930

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 174

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]10 20 02 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]02 00 20 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:00:34.950

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 156

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 00 01 58 0D 10 07 04
[8]02 85 8C 02 FA 09 1A 2B
[16]3C 0C 80 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 00 15 80 D1 00 70 40
[8]28 58 C0 2F A0 91 A2 B3
[16]C0 C8

#### PHY_DATA_IND

PHY MAC @ 00:00:34.960

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 157

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 00 D0 FF E1 D5 89 1A
[8]20 00 04 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 0D 0F FE 1D 58 91 A2
[8]00 00 40 00 00 00 00 00
[16]00 00

#### PHY_DATA_REQ

MAC PHY @ 00:00:34.970

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 178

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 02 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 20 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### CPHY_OUTSYNC_IND

PHY RRC @ 00:00:35.100

BTS unit: 1:1
Channel No: 0 Name: U_DPCH
CFN: 191

Message Details:

#### PHY_DATA_IND

PHY MAC @ 00:00:35.180

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 179

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 00 D0 FF E1 D5 89 1A
[8]20 00 04 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 0D 0F FE 1D 58 91 A2
[8]00 00 40 00 00 00 00 00
[16]00 00

#### PHY_DATA_REQ

MAC PHY @ 00:00:35.190

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 200

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 02 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 20 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### RLC_UM_DATA_REQ

RRC LLA @ 00:00:36.000

Channel ID: Rb1
Cell ID: -1

Message Details:

RLC_UM_DATA_REQ:

cellId:-1

routingInfo:

rB_Identity:1

uM_message:

dL_DCCH_Message:

integrityCheckInfo: Omit

message: (DL_DCCH_MessageType)

rrcConnectionRelease:

r3:

rrcConnectionRelease_r3: (RRCConnectionRelease_r3_IEs)

rrc_TransactionIdentifier:0
n_308:1
releaseCause:normalEvent

rplmn_information: Omit

laterNonCriticalExtensions: Omit

specialLI:false

#### PHY_DATA_REQ

MAC PHY @ 00:00:36.010

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 26

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]00 10 7F E3 C8 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:0
MAC SDU (144 bits):

[0]01 07 FE 3C 80 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### CRLC_Config_REQ

RRC LLA @ 00:00:37.020

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:1

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC_Config_CNF

LLA RRC @ 00:00:37.040

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:1

#### CRLC_Config_REQ

RRC LLA @ 00:00:37.040

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:2

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC_Config_CNF

LLA RRC @ 00:00:37.050

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:2

#### CRLC_Config_REQ

RRC LLA @ 00:00:37.050

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:3

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC_Config_CNF

LLA RRC @ 00:00:37.070

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:3

#### CRLC_Config_REQ

RRC LLA @ 00:00:37.070

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:4

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC_Config_CNF

LLA RRC @ 00:00:37.080

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:4

#### CRLC_Config_REQ

RRC LLA @ 00:00:37.080

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:1

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode)

dl_UM_RLC_Mode:

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):136

dl_RLCModeInfo: (UL_RLC_Mode)

ul_UM_RLC_Mode:

transmissionRLC_Discard:

timerBasedNoExplicit (NoExplicitDiscard):dt100

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity):1
dLlogicalChannelIdentity (LogicalChannelIdentity):1
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC_Config_CNF

LLA RRC @ 00:00:37.100

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:1

#### CRLC_Config_REQ

RRC LLA @ 00:00:37.100

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:2

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode)

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):128

dl_RLCModeInfo: (UL_RLC_Mode)

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity):2
dLlogicalChannelIdentity (LogicalChannelIdentity):2
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC_Config_CNF

LLA RRC @ 00:00:37.110

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:2

#### CRLC_Config_REQ

RRC LLA @ 00:00:37.110

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:3

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode)

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):128

dl_RLCModeInfo: (UL_RLC_Mode)

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity):3
dLlogicalChannelIdentity (LogicalChannelIdentity):3
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC_Config_CNF

LLA RRC @ 00:00:37.130

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:3

#### CRLC_Config_REQ

RRC LLA @ 00:00:37.130

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:4

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode)

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):128

dl_RLCModeInfo: (UL_RLC_Mode)

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity):4
dLlogicalChannelIdentity (LogicalChannelIdentity):4
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC_Config_CNF

LLA RRC @ 00:00:37.140

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:4

#### MMI_CmdReq

RRC LLA @ 00:00:37.140

Message Details:

MMI_CmdReq:

cmd (IA5String):Please switch on the UE

#### MMI_CmdCnf

LLA RRC @ 00:00:40.110

Message Details:

MMI_CmdCnf:

result:true
resultString (IA5String): Omit

#### PHY_DATA_IND

PHY MAC @ 00:00:52.470

BTS unit: 1:1
Channel No: 0 Name: U_RACH
CFN: 116

Message Details:

TFI:0
TB set size:168
TB size:168
TB set (raw):

[0]08 44 48 8C D1 00 04 02
[8]00 02 C0 00 00 00 00 00
[16]00 00 00 00 00 00

TB set (decoded):

TB 0:

TCTF:0
MAC SDU (166 bits):

[0]21 11 22 33 44 00 10 08
[8]00 0B 00 00 00 00 00 00
[16]00 00 00 00 00

#### RLC_TR_DATA_IND

LLA RRC @ 00:00:52.500

Channel ID: Rb0
Cell ID: 0

Message Details:

RLC_TR_DATA_IND:

cellId:0

routingInfo:

rB_Identity:0

tM_message:

uL_CCCH_Message:

integrityCheckInfo: Omit

message: (UL_CCCH_MessageType)

rrcConnectionRequest:

initialUE_Identity:

tmsi_and_LAI: (TMSI_and_LAI_GSM_MAP)

tmsi (TMSI_GSM_MAP):00010001001000100011001101000100

lai:

plmn_Identity:

mcc:

Digit:0
Digit:0
Digit:1

mnc:

Digit:0
Digit:1

lac:0000000000000001

establishmentCause:registration
protocolErrorIndicator:noError

measuredResultsOnRACH: Omit

v3d0NonCriticalExtensions: Omit

#### RLC_UM_DATA_REQ

RRC LLA @ 00:00:52.500

Channel ID: Rb0
Cell ID: 0

Message Details:

RLC_UM_DATA_REQ:

cellId:0

routingInfo:

rB_Identity:0

uM_message:

dL_CCCH_Message:

integrityCheckInfo: Omit

message: (DL_CCCH_MessageType)

rrcConnectionSetup:

r3:

rrcConnectionSetup_r3: (RRCConnectionSetup_r3_IEs)

initialUE_Identity:

tmsi_and_LAI: (TMSI_and_LAI_GSM_MAP)

tmsi (TMSI_GSM_MAP):00010001001000100011001101000100

lai:

plmn_Identity:

mcc:

Digit:0
Digit:0
Digit:1

mnc:

Digit:0
Digit:1

lac:0000000000000001

rrc_TransactionIdentifier:0
activationTime: Omit

new_U_RNTI: (U_RNTI)

srnc_Identity:000000000001
s_RNTI:00000000000000000001

new_c_RNTI (C_RNTI): Omit
rrc_StateIndicator:cell_DCH
utran_DRX_CycleLengthCoeff (UTRAN_DRX_CycleLengthCoefficient):9

capabilityUpdateRequirement:

ue_RadioCapabilityFDDUpdateRequirement:true
ue_RadioCapabilityTDDUpdateRequirement:false

systemSpecificCapUpdateReqList:

SystemSpecificCapUpdateReq:gsm

srb_InformationSetupList: (SRB_InformationSetupList2)

SRB_InformationSetup:

rb_Identity: Omit

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_UM_RLC_Mode:

transmissionRLC_Discard: Omit

dl_RLC_Mode:

dl_UM_RLC_Mode:

rb_MappingInfo:

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

dch (TransportChannelIdentity):5

logicalChannelIdentity:1

rlc_SizeList:

configured:

mac_LogicalChannelPriority:1

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

dch (TransportChannelIdentity):10

logicalChannelIdentity:1

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

rach:

logicalChannelIdentity:1

rlc_SizeList:

explicitList: (RLC_SizeExplicitList)

RLC_SizeInfo:

rlc_SizeIndex:1

mac_LogicalChannelPriority:1

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

fach:

logicalChannelIdentity:1

SRB_InformationSetup:

rb_Identity: Omit

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

rb_MappingInfo:

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

dch (TransportChannelIdentity):5

logicalChannelIdentity:2

rlc_SizeList:

configured:

mac_LogicalChannelPriority:2

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

dch (TransportChannelIdentity):10

logicalChannelIdentity:2

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

rach:

logicalChannelIdentity:2

rlc_SizeList:

explicitList: (RLC_SizeExplicitList)

RLC_SizeInfo:

rlc_SizeIndex:1

mac_LogicalChannelPriority:2

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

fach:

logicalChannelIdentity:2

SRB_InformationSetup:

rb_Identity: Omit

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

rb_MappingInfo:

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

dch (TransportChannelIdentity):5

logicalChannelIdentity:3

rlc_SizeList:

configured:

mac_LogicalChannelPriority:3

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

dch (TransportChannelIdentity):10

logicalChannelIdentity:3

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

rach:

logicalChannelIdentity:3

rlc_SizeList:

explicitList: (RLC_SizeExplicitList)

RLC_SizeInfo:

rlc_SizeIndex:1

mac_LogicalChannelPriority:3

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

fach:

logicalChannelIdentity:3

SRB_InformationSetup:

rb_Identity: Omit

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

rb_MappingInfo:

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

dch (TransportChannelIdentity):5

logicalChannelIdentity:4

rlc_SizeList:

configured:

mac_LogicalChannelPriority:4

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

dch (TransportChannelIdentity):10

logicalChannelIdentity:4

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

rach:

logicalChannelIdentity:4

rlc_SizeList:

explicitList: (RLC_SizeExplicitList)

RLC_SizeInfo:

rlc_SizeIndex:1

mac_LogicalChannelPriority:4

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

fach:

logicalChannelIdentity:4

ul_CommonTransChInfo:

tfc_Subset: Omit

prach_TFCS: (TFCS) Omit

modeSpecificInfo:

fdd:

ul_TFCS: (TFCS)

normalTFCI_Signalling: (ExplicitTFCS_Configuration)

complete: (TFCS_ReconfAdd)

ctfcSize:

ctfc2Bit:

:

ctfc2:0

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc2:1

powerOffsetInformation:

gainFactorInformation:

signalledGainFactors:

modeSpecificInfo:

fdd:

gainFactorBetaC (GainFactor):11

gainFactorBetaD (GainFactor):15
referenceTFC_ID:0

powerOffsetPp_m: Omit

ul_AddReconfTransChInfoList:

UL_AddReconfTransChInformation:

ul_TransportChannelType (UL_TrCH_Type):dch
transportChannelIdentity:5

transportFormatSet:

dedicatedTransChTFS:

tti:

tti10: (DedicatedDynamicTF_InfoList)

DedicatedDynamicTF_Info:

rlc_Size:

bitMode: (BitModeRLC_SizeInfo)

sizeType2:

part1:2
part2: Omit

numberOfTbSizeList:

NumberOfTransportBlocks:

zero:

NumberOfTransportBlocks:

one:

logicalChannelList:

allSizes:

semistaticTF_Information:

channelCodingType:

convolutional (CodingRate):third

rateMatchingAttribute:192
crc_Size:crc16

dl_CommonTransChInfo:

sccpch_TFCS: (TFCS) Omit

modeSpecificInfo:

fdd:

dl_Parameters:

sameAsUL:

dl_AddReconfTransChInfoList:

DL_AddReconfTransChInformation:

dl_TransportChannelType (DL_TrCH_Type):dch
dl_transportChannelIdentity (TransportChannelIdentity):10

tfs_SignallingMode:

sameAsULTrCH: (UL_TransportChannelIdentity)

ul_TransportChannelType (UL_TrCH_Type):dch
ul_TransportChannelIdentity (TransportChannelIdentity):5

dch_QualityTarget: (QualityTarget)

bler_QualityValue:-20

dummy: (TM_SignallingInfo) Omit

frequencyInfo: Omit

maxAllowedUL_TX_Power: Omit

ul_ChannelRequirement:

ul_DPCH_Info:

ul_DPCH_PowerControlInfo:

fdd:

dpcch_PowerOffset:-40
pc_Preamble:1
sRB_delay:7

powerControlAlgorithm:

algorithm1 (TPC_StepSizeFDD):0

modeSpecificInfo:

fdd:

scramblingCodeType:longSC
scramblingCode (UL_ScramblingCode):0
numberOfDPDCH: Omit
spreadingFactor:sf64
tfci_Existence:true
numberOfFBI_Bits: Omit
puncturingLimit:pl1

dl_CommonInformation:

dl_DPCH_InfoCommon:

cfnHandling:

initialise:

cfntargetsfnframeoffset: Omit

modeSpecificInfo:

fdd:

dl_DPCH_PowerControlInfo:

modeSpecificInfo:

fdd:

dpc_Mode:singleTPC

powerOffsetPilot_pdpdch:0

dl_rate_matching_restriction: Omit

spreadingFactorAndPilot: (SF512_AndPilot)

sfd128 (PilotBits128):pb4

positionFixedOrFlexible:fixed
tfci_Existence:false

modeSpecificInfo:

fdd:

defaultDPCH_OffsetValue (DefaultDPCH_OffsetValueFDD):0

dpch_CompressedModeInfo: Omit

tx_DiversityMode:noDiversity

ssdt_Information: Omit

dl_InformationPerRL_List:

DL_InformationPerRL:

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode:100

pdsch_SHO_DCH_Info: Omit

pdsch_CodeMapping: Omit

dl_DPCH_InfoPerRL:

fdd:

pCPICH_UsageForChannelEst:mayBeUsed
dpch_FrameOffset:0

secondaryCPICH_Info: Omit

dl_ChannelisationCodeList:

DL_ChannelisationCode:

secondaryScramblingCode:1

sf_AndCodeNumber: (SF512_AndCodeNumber)

sf128:0

scramblingCodeChange:noCodeChange

tpc_CombinationIndex:0
ssdt_CellIdentity: Omit
closedLoopTimingAdjMode: Omit

sccpch_InfoforFACH: Omit

laterNonCriticalExtensions: Omit

specialLI:true

#### PHY_DATA_REQ

MAC PHY @ 00:00:52.540

BTS unit: 1:1
Channel No: 0 Name: FACH
CFN: 143

Message Details:

TFI:2
TB set size:336
TB size:168
TB set (raw, each TB word aligned):

[0]40 19 F8 30 E7 22 24 46
[8]68 80 02 01 00 01 00 04
[16]00 00 4D 82 69 00 40 1A
[24]3A 10 10 89 0D 42 00 02
[32]81 9E 8E 46 C9 A6 7C 9C
[40]4E 74 20 00

TB set (decoded):

TB 0:

TCTF:64
MAC SDU (160 bits):

[0]19 F8 30 E7 22 24 46 68
[8]80 02 01 00 01 00 04 00
[16]00 4D 82 69

TB 1:

TCTF:64
MAC SDU (160 bits):

[0]1A 3A 10 10 89 0D 42 00
[8]02 81 9E 8E 46 C9 A6 7C
[16]9C 4E 74 20

#### PHY_DATA_REQ

MAC PHY @ 00:00:52.550

BTS unit: 1:1
Channel No: 0 Name: FACH
CFN: 144

Message Details:

TFI:2
TB set size:336
TB size:168
TB set (raw, each TB word aligned):

[0]40 1C A5 12 3A 8C 00 15
[8]13 3D 1C 8D 93 4C F9 38
[16]9C E8 42 52 24 00 40 1E
[24]B5 28 00 4A 46 7A 39 1B
[32]26 99 F2 71 39 D0 86 B4
[40]49 EA 70 00

TB set (decoded):

TB 0:

TCTF:64
MAC SDU (160 bits):

[0]1C A5 12 3A 8C 00 15 13
[8]3D 1C 8D 93 4C F9 38 9C
[16]E8 42 52 24

TB 1:

TCTF:64
MAC SDU (160 bits):

[0]1E B5 28 00 4A 46 7A 39
[8]1B 26 99 F2 71 39 D0 86
[16]B4 49 EA 70

#### PHY_DATA_REQ

MAC PHY @ 00:00:52.560

BTS unit: 1:1
Channel No: 0 Name: FACH
CFN: 145

Message Details:

TFI:2
TB set size:336
TB size:168
TB set (raw, each TB word aligned):

[0]40 20 00 D4 C8 00 06 25
[8]2B F0 02 00 08 82 23 BF
[16]66 08 98 95 A5 00 40 23
[24]23 FE 47 82 00 00 01 3F
[32]90 0A 14 00 02 06 40 00
[40]0C 28 08 00

TB set (decoded):

TB 0:

TCTF:64
MAC SDU (160 bits):

[0]20 00 D4 C8 00 06 25 2B
[8]F0 02 00 08 82 23 BF 66
[16]08 98 95 A5

TB 1:

TCTF:64
MAC SDU (160 bits):

[0]23 23 FE 47 82 00 00 01
[8]3F 90 0A 14 00 02 06 40
[16]00 0C 28 08

#### CPHY_SYNC_IND

PHY RRC @ 00:00:52.810

BTS unit: 1:1
Channel No: 0 Name: U_DPCH
CFN: 170

Message Details:

#### PHY_DATA_IND

PHY MAC @ 00:00:52.990

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 168

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 00 04 A0 80 00 5A 00
[8]00 59 1A 85 50 6A 4C 26
[16]84 62 C0 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 00 4A 08 00 05 A0 00
[8]05 91 A8 55 06 A4 C2 68
[16]46 2C

#### PHY_DATA_IND

PHY MAC @ 00:00:53.000

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 169

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 00 D1 5F E9 40 20 80
[8]00 80 01 18 A1 40 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 0D 15 FE 94 02 08 00
[8]08 00 11 8A 14 00 00 00
[16]00 00

#### PHY_DATA_REQ

MAC PHY @ 00:00:53.010

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 190

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]10 20 02 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]02 00 20 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### RLC_AM_DATA_IND

LLA RRC @ 00:00:53.020

Channel ID: Rb2
Cell ID: -1

Message Details:

RLC_AM_DATA_IND:

cellId:-1

routingInfo:

rB_Identity:2

integrityResult:

integrityUsed (IntegrityStatus):i_pass

aM_message:

uL_DCCH_Message:

integrityCheckInfo: Omit

message: (UL_DCCH_MessageType)

rrcConnectionSetupComplete:

rrc_TransactionIdentifier:0

startList:

STARTSingle:

cn_DomainIdentity:cs_domain
start_Value:00000000000000010110

STARTSingle:

cn_DomainIdentity:ps_domain
start_Value:00000000000000000010

ue_RadioAccessCapability:

accessStratumReleaseIndicator:r99

pdcp_Capability:

losslessSRNS_RelocationSupport:true

supportForRfc2507:

notSupported:

rlc_Capability:

totalRLC_AM_BufferSize:kb50
maximumRLC_WindowSize:mws2047
maximumAM_EntityNumber (MaximumAM_EntityNumberRLC_Cap):am6

transportChannelCapability:

dl_TransChCapability:

maxNoBitsReceived (MaxNoBits):b6400
maxConvCodeBitsReceived (MaxNoBits):b640

turboDecodingSupport: (TurboSupport)

supported (MaxNoBits):b6400

maxSimultaneousTransChs (MaxSimultaneousTransChsDL):e8
maxSimultaneousCCTrCH_Count:1
maxReceivedTransportBlocks (MaxTransportBlocksDL):tb32
maxNumberOfTFC (MaxNumberOfTFC_DL):tfc128
maxNumberOfTF:tf64

ul_TransChCapability:

maxNoBitsTransmitted (MaxNoBits):b3840
maxConvCodeBitsTransmitted (MaxNoBits):b640

turboEncodingSupport: (TurboSupport)

supported (MaxNoBits):b3840

maxSimultaneousTransChs (MaxSimultaneousTransChsUL):e8

modeSpecificInfo:

fdd:

maxTransmittedBlocks (MaxTransportBlocksUL):tb8
maxNumberOfTFC (MaxNumberOfTFC_UL):tfc32
maxNumberOfTF:tf32

rf_Capability:

fddRF_Capability:

ue_PowerClass:4
txRxFrequencySeparation:mhz190

tddRF_Capability: Omit

physicalChannelCapability:

fddPhysChCapability:

downlinkPhysChCapability: (DL_PhysChCapabilityFDD)

maxNoDPCH_PDSCH_Codes:3
maxNoPhysChBitsReceived:b19200
supportForSF_512:false
supportOfPDSCH:false

simultaneousSCCPCH_DPCH_Reception:

notSupported:

uplinkPhysChCapability: (UL_PhysChCapabilityFDD)

maxNoDPDCH_BitsTransmitted:b2400
supportOfPCPCH:false

tddPhysChCapability: Omit

ue_MultiModeRAT_Capability:

multiRAT_CapabilityList: (MultiRAT_Capability)

supportOfGSM:false
supportOfMulticarrier:false

multiModeCapability:fdd

securityCapability:

cipheringAlgorithmCap:0000000000000001
integrityProtectionAlgorithmCap:0000000000000010

ue_positioning_Capability:

standaloneLocMethodsSupported:false
ue_BasedOTDOA_Supported:false
networkAssistedGPS_Supported:noNetworkAssistedGPS
supportForUE_GPS_TimingOfCellFrames:false
supportForIPDL:false

measurementCapability:

downlinkCompressedMode: (CompressedModeMeasCapability)

fdd_Measurements:true
tdd_Measurements: Omit

gsm_Measurements:

gsm900:false
dcs1800:false
gsm1900:false

multiCarrierMeasurements: Omit

uplinkCompressedMode: (CompressedModeMeasCapability)

fdd_Measurements:true
tdd_Measurements: Omit

gsm_Measurements:

gsm900:false
dcs1800:false
gsm1900:false

multiCarrierMeasurements: Omit

ue_RATSpecificCapability: (InterRAT_UE_RadioAccessCapabilityList) Omit

v370NonCriticalExtensions: Omit

#### PHY_DATA_IND

PHY MAC @ 00:00:53.220

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 191

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 00 D1 5F E9 40 20 80
[8]00 80 01 18 A1 40 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 0D 15 FE 94 02 08 00
[8]08 00 11 8A 14 00 00 00
[16]00 00

#### PHY_DATA_REQ

MAC PHY @ 00:00:53.230

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 212

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]10 20 02 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]02 00 20 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:00:53.250

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 194

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 00 01 58 0D 10 0C 84
[8]00 81 62 80 01 86 01 82
[16]FA 09 10 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 00 15 80 D1 00 C8 40
[8]08 16 28 00 18 60 18 2F
[16]A0 91

#### PHY_DATA_IND

PHY MAC @ 00:00:53.260

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 195

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 00 8A 2B 3C 00 78 88
[8]00 00 82 82 A1 67 00 02
[16]00 20 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 08 A2 B3 C0 07 88 80
[8]00 08 28 2A 16 70 00 20
[16]02 00

#### PHY_DATA_IND

PHY MAC @ 00:00:53.270

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 196

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 01 50 5F E0 04 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 15 05 FE 00 40 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_REQ

MAC PHY @ 00:00:53.280

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 217

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 03 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_REQ

MAC PHY @ 00:00:53.310

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 220

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 00 01 42 04 E1 02 40
[8]26 04 2A AA AA AA AA AA
[16]AA AA A0 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 00 14 20 4E 10 24 02
[8]60 42 AA AA AA AA AA AA
[16]AA AA

#### PHY_DATA_REQ

MAC PHY @ 00:00:53.320

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 221

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 00 8A AA AA AA AA AA
[8]AA AA B0 25 02 0C C2 20
[16]06 64 50 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 08 AA AA AA AA AA AA
[8]AA AB 02 50 20 CC 22 00
[16]66 45

#### PHY_DATA_REQ

MAC PHY @ 00:00:53.330

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 222

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 01 51 7F EB A0 00 0A
[8]A8 8E EC C2 20 06 64 40
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 15 17 FE BA 00 00 AA
[8]88 EE CC 22 00 66 44 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:00:53.490

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 218

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 01 50 5F E0 04 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 15 05 FE 00 40 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_REQ

MAC PHY @ 00:00:53.500

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 239

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 03 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_REQ

MAC PHY @ 00:00:53.510

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 240

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 01 51 7F EB A0 00 0A
[8]A8 8E EC C2 20 06 64 40
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 15 17 FE BA 00 00 AA
[8]88 EE CC 22 00 66 44 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:00:53.570

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 226

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 03 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:00:53.780

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 247

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 01 86 C8 06 84 09 81
[8]91 2A A2 3B B3 14 82 08
[16]80 19 90 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 18 6C 80 68 40 98 19
[8]12 AA 23 BB 31 48 20 88
[16]01 99

#### PHY_DATA_IND

PHY MAC @ 00:00:53.790

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 248

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 03 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:00:53.800

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 249

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 02 50 3F E1 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 25 03 FE 10 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_REQ

MAC PHY @ 00:00:53.810

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 14

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 05 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 50 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### CRLC_SecurityMode_Config_REQ

RRC LLA @ 00:00:53.820

Cell ID: -1

Message Details:

CRLC_SecurityMode_Config_REQ:

cellId:-1

rlcSecurityInfo: (SecurityInfo)

cn_DomainIdentity:ps_domain
startValue (START_Value):00000000000000000000
cipheringKey: Omit
integrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
gsmCipheringKey: Omit

#### CRLC_SecurityMode_Config_CNF

LLA RRC @ 00:00:53.830

Cell ID: -1

Message Details:

CRLC_SecurityMode_Config_CNF:

cellId:-1

#### CRLC_SetRRC_MessageSN_REQ

RRC LLA @ 00:00:53.830

Channel ID: Rb0
Cell ID: 0

Message Details:

CRLC_SetRRC_MessageSN_REQ:

cellId:0

routingInfo:

rB_Identity:0

count_I_LSB_UL (RRC_SequenceNumber): Omit
count_I_LSB_DL (RRC_SequenceNumber):0

#### CRLC_SetRRC_MessageSN_CNF

LLA RRC @ 00:00:53.850

Channel ID: Rb0
Cell ID: 0

Message Details:

CRLC_SetRRC_MessageSN_CNF:

cellId:0

routingInfo:

rB_Identity:0

#### CRLC_SetRRC_MessageSN_REQ

RRC LLA @ 00:00:53.850

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_REQ:

cellId:-1

routingInfo:

rB_Identity:1

count_I_LSB_UL (RRC_SequenceNumber): Omit
count_I_LSB_DL (RRC_SequenceNumber):0

#### CRLC_SetRRC_MessageSN_CNF

LLA RRC @ 00:00:53.860

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_CNF:

cellId:-1

routingInfo:

rB_Identity:1

#### CRLC_SetRRC_MessageSN_REQ

RRC LLA @ 00:00:53.860

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_REQ:

cellId:-1

routingInfo:

rB_Identity:2

count_I_LSB_UL (RRC_SequenceNumber): Omit
count_I_LSB_DL (RRC_SequenceNumber):0

#### CRLC_SetRRC_MessageSN_CNF

LLA RRC @ 00:00:53.880

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_CNF:

cellId:-1

routingInfo:

rB_Identity:2

#### CRLC_SetRRC_MessageSN_REQ

RRC LLA @ 00:00:53.880

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_REQ:

cellId:-1

routingInfo:

rB_Identity:3

count_I_LSB_UL (RRC_SequenceNumber): Omit
count_I_LSB_DL (RRC_SequenceNumber):0

#### CRLC_SetRRC_MessageSN_CNF

LLA RRC @ 00:00:53.890

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_CNF:

cellId:-1

routingInfo:

rB_Identity:3

#### CRLC_SetRRC_MessageSN_REQ

RRC LLA @ 00:00:53.890

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_REQ:

cellId:-1

routingInfo:

rB_Identity:4

count_I_LSB_UL (RRC_SequenceNumber): Omit
count_I_LSB_DL (RRC_SequenceNumber):0

#### CRLC_SetRRC_MessageSN_CNF

LLA RRC @ 00:00:53.910

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_CNF:

cellId:-1

routingInfo:

rB_Identity:4

#### CRLC_Integrity_Activate_REQ

RRC LLA @ 00:00:53.910

Cell ID: -1

Message Details:

CRLC_Integrity_Activate_REQ:

cellId:-1
cn_DomainIdentity:ps_domain

integrityActivationInfo:

integrityProtectionModeInfo:

integrityProtectionModeCommand:

startIntegrityProtection:

integrityProtInitNumber:00001111000011110000111100001111

integrityProtectionAlgorithm:uia1

#### CRLC_Integrity_Activate_CNF

LLA RRC @ 00:00:53.930

Cell ID: -1

Message Details:

CRLC_Integrity_Activate_CNF:

cellId:-1

#### CRLC_Integrity_Activate_REQ

RRC LLA @ 00:00:53.930

Cell ID: -1

Message Details:

CRLC_Integrity_Activate_REQ:

cellId:-1
cn_DomainIdentity:ps_domain

integrityActivationInfo:

ul_IntegProtActivationInfo: (IntegrityProtActivationInfoList)

SS_IntegrityProtActivationTimeInfo:

rb_Identity:2
rrc_MessageSequenceNumber:0

#### CMAC Integrity Check Request

RRC MAC @ 00:00:53.940

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000001
Data:

[0]00 00 00 01
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:1 (RNC to UE)
Message Length (bits):128
Message:

[0]80 00 00 01 04 06 00 00
[8]80 01 41 E1 E1 E1 F0 00

#### CMAC Integrity Check Result

MAC RRC @ 00:00:53.940

Message Details:

Integrity Check Result:

MAC-I:11101000011101111000001101000000
Data:

[0]E8 77 83 40

#### CRLC_Integrity_Activate_CNF

LLA RRC @ 00:00:53.940

Cell ID: -1

Message Details:

CRLC_Integrity_Activate_CNF:

cellId:-1

#### RLC_AM_DATA_REQ

RRC LLA @ 00:00:53.940

Channel ID: Rb2
Cell ID: -1

Message Details:

RLC_AM_DATA_REQ:

cellId:-1

routingInfo:

rB_Identity:2

confirmationRequest: (AmConfirmationRequest)

noConfirmationRequest:

aM_message:

dL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode:00000000000000000000000000000000
rrc_MessageSequenceNumber:0

message: (DL_DCCH_MessageType)

securityModeCommand:

r3:

securityModeCommand_r3: (SecurityModeCommand_r3_IEs)

rrc_TransactionIdentifier:0

securityCapability:

cipheringAlgorithmCap:0000000000000001
integrityProtectionAlgorithmCap:0000000000000010

cipheringModeInfo: Omit

integrityProtectionModeInfo:

integrityProtectionModeCommand:

startIntegrityProtection:

integrityProtInitNumber:00001111000011110000111100001111

integrityProtectionAlgorithm:uia1

cn_DomainIdentity:ps_domain

ue_SystemSpecificSecurityCap: (InterRAT_UE_SecurityCapList)

InterRAT_UE_SecurityCapability:

gsm:

gsmSecurityCapability:0000000

laterNonCriticalExtensions: Omit

#### PHY_DATA_REQ

MAC PHY @ 00:00:53.950

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 28

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 00 0F 43 BC 1A 00 C0
[8]60 00 08 00 14 1E 1E 1E
[16]1F 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 00 F4 3B C1 A0 0C 06
[8]00 00 80 01 41 E1 E1 E1
[16]F0 00

#### PHY_DATA_REQ

MAC PHY @ 00:00:53.960

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 29

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 00 D0 1F E0 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 0D 01 FE 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:00:54.020

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 15

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 02 50 3F E1 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 25 03 FE 10 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_REQ

MAC PHY @ 00:00:54.030

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 36

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 05 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 50 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_REQ

MAC PHY @ 00:00:54.150

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 48

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 00 D0 1F E0 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 0D 01 FE 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:00:54.200

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 33

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]10 20 02 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]02 00 20 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:00:54.210

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 34

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 01 51 3F EC 59 1B E7
[8]10 D2 10 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 15 13 FE C5 91 BE 71
[8]0D 21 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_REQ

MAC PHY @ 00:00:54.220

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 55

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]10 20 03 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### CMAC Integrity Check Request

RRC MAC @ 00:00:54.240

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000001
Data:

[0]00 00 00 01
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:0 (UE to RNC)
Message Length (bits):72
Message:

[0]80 00 00 01 05 21 00 00
[8]00

#### CMAC Integrity Check Result

MAC RRC @ 00:00:54.240

Message Details:

Integrity Check Result:

MAC-I:10001011001000110111110011100010
Data:

[0]8B 23 7C E2

#### RLC_AM_DATA_IND

LLA RRC @ 00:00:54.240

Channel ID: Rb2
Cell ID: -1

Message Details:

RLC_AM_DATA_IND:

cellId:-1

routingInfo:

rB_Identity:2

integrityResult:

integrityUsed (IntegrityStatus):i_pass

aM_message:

uL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode:10001011001000110111110011100010
rrc_MessageSequenceNumber:1

message: (UL_DCCH_MessageType)

securityModeComplete:

rrc_TransactionIdentifier:0

ul_IntegProtActivationInfo: (IntegrityProtActivationInfo)

rrc_MessageSequenceNumberList:

RRC_MessageSequenceNumber:0
RRC_MessageSequenceNumber:0
RRC_MessageSequenceNumber:0
RRC_MessageSequenceNumber:0
RRC_MessageSequenceNumber:0

rb_UL_CiphActivationTimeInfo: (RB_ActivationTimeInfoList) Omit

laterNonCriticalExtensions: Omit

#### CRLC_Integrity_Activate_REQ

RRC LLA @ 00:00:54.240

Cell ID: -1

Message Details:

CRLC_Integrity_Activate_REQ:

cellId:-1
cn_DomainIdentity:ps_domain

integrityActivationInfo:

ul_IntegProtActivationInfo: (IntegrityProtActivationInfoList)

SS_IntegrityProtActivationTimeInfo:

rb_Identity:0
rrc_MessageSequenceNumber:0

SS_IntegrityProtActivationTimeInfo:

rb_Identity:1
rrc_MessageSequenceNumber:0

SS_IntegrityProtActivationTimeInfo:

rb_Identity:3
rrc_MessageSequenceNumber:0

SS_IntegrityProtActivationTimeInfo:

rb_Identity:4
rrc_MessageSequenceNumber:0

#### CMAC Integrity Check Request

RRC MAC @ 00:00:54.250

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000001
Data:

[0]00 00 00 01
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:1 (RNC to UE)
Message Length (bits):240
Message:

[0]80 00 00 01 81 42 02 A1
[8]00 40 64 C0 80 1E 22 00
[16]00 20 A3 35 62 46 E3 00
[24]BE 81 30 EC A8 60

#### CMAC Integrity Check Result

MAC RRC @ 00:00:54.250

Message Details:

Integrity Check Result:

MAC-I:01010011010110111100110000111101
Data:

[0]53 5B CC 3D

#### CRLC_Integrity_Activate_CNF

LLA RRC @ 00:00:54.250

Cell ID: -1

Message Details:

CRLC_Integrity_Activate_CNF:

cellId:-1

#### PHY_DATA_REQ

MAC PHY @ 00:00:54.270

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 60

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 01 8A 9A DE 61 E8 94
[8]20 2A 10 04 06 4C 08 01
[16]E2 20 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 18 A9 AD E6 1E 89 42
[8]02 A1 00 40 64 C0 80 1E
[16]22 00

#### PHY_DATA_REQ

MAC PHY @ 00:00:54.280

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 61

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 02 51 DF E0 02 0A 33
[8]56 24 6E 30 0B E8 13 0E
[16]CA 86 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 25 1D FE 00 20 A3 35
[8]62 46 E3 00 BE 81 30 EC
[16]A8 60

#### PHY_DATA_IND

PHY MAC @ 00:00:54.420

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 55

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]10 20 02 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]02 00 20 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:00:54.430

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 56

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 01 51 3F EC 59 1B E7
[8]10 D2 10 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 15 13 FE C5 91 BE 71
[8]0D 21 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_REQ

MAC PHY @ 00:00:54.440

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 77

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]10 20 03 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_REQ

MAC PHY @ 00:00:54.470

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 80

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 02 51 DF E0 02 0A 33
[8]56 24 6E 30 0B E8 13 0E
[16]CA 86 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 25 1D FE 00 20 A3 35
[8]62 46 E3 00 BE 81 30 EC
[16]A8 60

#### PHY_DATA_IND

PHY MAC @ 00:00:54.520

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 65

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 05 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 50 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:00:54.530

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 66

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 02 D1 5F ED 6F 6F 71
[8]E0 EC 80 08 40 18 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 2D 15 FE D6 F6 F7 1E
[8]0E C8 00 84 01 80 00 00
[16]00 00

#### PHY_DATA_REQ

MAC PHY @ 00:00:54.540

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 87

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 06 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 60 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### CMAC Integrity Check Request

RRC MAC @ 00:00:54.550

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000001
Data:

[0]00 00 00 01
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:0 (UE to RNC)
Message Length (bits):80
Message:

[0]80 00 00 01 86 C8 00 84
[8]01 80

#### CMAC Integrity Check Result

MAC RRC @ 00:00:54.550

Message Details:

Integrity Check Result:

MAC-I:10101101111011011110111000111100
Data:

[0]AD ED EE 3C

#### PHY_DATA_IND

PHY MAC @ 00:00:54.740

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 87

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 05 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 50 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:00:54.750

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 88

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 02 D1 5F ED 6F 6F 71
[8]E0 EC 80 08 40 18 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 2D 15 FE D6 F6 F7 1E
[8]0E C8 00 84 01 80 00 00
[16]00 00

#### PHY_DATA_REQ

MAC PHY @ 00:00:54.760

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 109

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 06 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 60 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### CMAC Integrity Check Request

RRC MAC @ 00:00:55.570

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000001
Data:

[0]00 00 00 01
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:1 (RNC to UE)
Message Length (bits):56
Message:

[0]80 00 00 00 83 C8 00

#### CMAC Integrity Check Result

MAC RRC @ 00:00:55.570

Message Details:

Integrity Check Result:

MAC-I:11101100100111000001011111010011
Data:

[0]EC 9C 17 D3

#### RLC_UM_DATA_REQ

RRC LLA @ 00:00:55.570

Channel ID: Rb1
Cell ID: -1

Message Details:

RLC_UM_DATA_REQ:

cellId:-1

routingInfo:

rB_Identity:1

uM_message:

dL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode:00000000000000000000000000000000
rrc_MessageSequenceNumber:0

message: (DL_DCCH_MessageType)

rrcConnectionRelease:

r3:

rrcConnectionRelease_r3: (RRCConnectionRelease_r3_IEs)

rrc_TransactionIdentifier:0
n_308:1
releaseCause:normalEvent

rplmn_information: Omit

laterNonCriticalExtensions: Omit

specialLI:false

#### PHY_DATA_REQ

MAC PHY @ 00:00:55.580

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 191

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]00 10 FF EF 64 E0 BE 98
[8]BC 80 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:0
MAC SDU (144 bits):

[0]01 0F FE F6 4E 0B E9 8B
[8]C8 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:00:55.820

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 195

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]00 10 DF EF BF 16 16 70
[8]C4 00 B0 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:0
MAC SDU (144 bits):

[0]01 0D FE FB F1 61 67 0C
[8]40 0B 00 00 00 00 00 00
[16]00 00

#### CMAC Integrity Check Request

RRC MAC @ 00:00:55.830

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000001
Data:

[0]00 00 00 01
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:0 (UE to RNC)
Message Length (bits):48
Message:

[0]80 00 00 00 84 40

#### CMAC Integrity Check Result

MAC RRC @ 00:00:55.830

Message Details:

Integrity Check Result:

MAC-I:11110111111000101100001011001110
Data:

[0]F7 E2 C2 CE

#### RLC_UM_DATA_IND

LLA RRC @ 00:00:55.830

Channel ID: Rb1
Cell ID: -1

Message Details:

RLC_UM_DATA_IND:

cellId:-1

routingInfo:

rB_Identity:1

integrityResult:

integrityUsed (IntegrityStatus):i_pass

uM_message:

uL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode:11110111111000101100001011001110
rrc_MessageSequenceNumber:1

message: (UL_DCCH_MessageType)

rrcConnectionReleaseComplete:

rrc_TransactionIdentifier:0

errorIndication: (FailureCauseWithProtErr) Omit

laterNonCriticalExtensions: Omit

#### PHY_DATA_IND

PHY MAC @ 00:00:55.980

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 211

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]00 30 DF ED CD 18 3E 01
[8]44 00 B0 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:0
MAC SDU (144 bits):

[0]03 0D FE DC D1 83 E0 14
[8]40 0B 00 00 00 00 00 00
[16]00 00

#### CMAC Integrity Check Request

RRC MAC @ 00:00:56.000

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000010
Data:

[0]00 00 00 02
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:0 (UE to RNC)
Message Length (bits):48
Message:

[0]80 00 00 00 84 40

#### CMAC Integrity Check Result

MAC RRC @ 00:00:56.000

Message Details:

Integrity Check Result:

MAC-I:10111001101000110000011111000000
Data:

[0]B9 A3 07 C0

#### RLC_UM_DATA_IND

LLA RRC @ 00:00:56.000

Channel ID: Rb1
Cell ID: -1

Message Details:

RLC_UM_DATA_IND:

cellId:-1

routingInfo:

rB_Identity:1

integrityResult:

integrityUsed (IntegrityStatus):i_pass

uM_message:

uL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode:10111001101000110000011111000000
rrc_MessageSequenceNumber:2

message: (UL_DCCH_MessageType)

rrcConnectionReleaseComplete:

rrc_TransactionIdentifier:0

errorIndication: (FailureCauseWithProtErr) Omit

laterNonCriticalExtensions: Omit

#### CRLC_Config_REQ

RRC LLA @ 00:00:56.000

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:1

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC_Config_CNF

LLA RRC @ 00:00:56.020

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:1

#### CRLC_Config_REQ

RRC LLA @ 00:00:56.020

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:2

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CPHY_OUTSYNC_IND

PHY RRC @ 00:00:56.030

BTS unit: 1:1
Channel No: 0 Name: U_DPCH
CFN: 236

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:00:56.040

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:2

#### CRLC_Config_REQ

RRC LLA @ 00:00:56.040

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:3

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC_Config_CNF

LLA RRC @ 00:00:56.050

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:3

#### CRLC_Config_REQ

RRC LLA @ 00:00:56.050

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:4

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC_Config_CNF

LLA RRC @ 00:00:56.070

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:4

#### CRLC_Config_REQ

RRC LLA @ 00:00:56.070

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:1

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode)

dl_UM_RLC_Mode:

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):136

dl_RLCModeInfo: (UL_RLC_Mode)

ul_UM_RLC_Mode:

transmissionRLC_Discard:

timerBasedNoExplicit (NoExplicitDiscard):dt100

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity):1
dLlogicalChannelIdentity (LogicalChannelIdentity):1
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC_Config_CNF

LLA RRC @ 00:00:56.080

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:1

#### CRLC_Config_REQ

RRC LLA @ 00:00:56.080

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:2

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode)

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):128

dl_RLCModeInfo: (UL_RLC_Mode)

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity):2
dLlogicalChannelIdentity (LogicalChannelIdentity):2
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC_Config_CNF

LLA RRC @ 00:00:56.100

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:2

#### CRLC_Config_REQ

RRC LLA @ 00:00:56.100

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:3

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode)

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):128

dl_RLCModeInfo: (UL_RLC_Mode)

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity):3
dLlogicalChannelIdentity (LogicalChannelIdentity):3
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC_Config_CNF

LLA RRC @ 00:00:56.110

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:3

#### CRLC_Config_REQ

RRC LLA @ 00:00:56.110

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:4

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode)

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):128

dl_RLCModeInfo: (UL_RLC_Mode)

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity):4
dLlogicalChannelIdentity (LogicalChannelIdentity):4
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC_Config_CNF

LLA RRC @ 00:00:56.130

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:4

#### PHY_DATA_IND

PHY MAC @ 00:06:56.410

BTS unit: 1:1
Channel No: 0 Name: U_RACH
CFN: 158

Message Details:

TFI:0
TB set size:168
TB size:168
TB set (raw):

[0]08 44 48 8C D1 00 04 02
[8]00 02 C0 00 00 00 00 00
[16]00 00 00 00 00 00

TB set (decoded):

TB 0:

TCTF:0
MAC SDU (166 bits):

[0]21 11 22 33 44 00 10 08
[8]00 0B 00 00 00 00 00 00
[16]00 00 00 00 00

#### RLC_TR_DATA_IND

LLA RRC @ 00:06:56.440

Channel ID: Rb0
Cell ID: 0

Message Details:

RLC_TR_DATA_IND:

cellId:0

routingInfo:

rB_Identity:0

tM_message:

uL_CCCH_Message:

integrityCheckInfo: Omit

message: (UL_CCCH_MessageType)

rrcConnectionRequest:

initialUE_Identity:

tmsi_and_LAI: (TMSI_and_LAI_GSM_MAP)

tmsi (TMSI_GSM_MAP):00010001001000100011001101000100

lai:

plmn_Identity:

mcc:

Digit:0
Digit:0
Digit:1

mnc:

Digit:0
Digit:1

lac:0000000000000001

establishmentCause:registration
protocolErrorIndicator:noError

measuredResultsOnRACH: Omit

v3d0NonCriticalExtensions: Omit

#### RLC_UM_DATA_REQ

RRC LLA @ 00:06:56.440

Channel ID: Rb0
Cell ID: 0

Message Details:

RLC_UM_DATA_REQ:

cellId:0

routingInfo:

rB_Identity:0

uM_message:

dL_CCCH_Message:

integrityCheckInfo: Omit

message: (DL_CCCH_MessageType)

rrcConnectionSetup:

r3:

rrcConnectionSetup_r3: (RRCConnectionSetup_r3_IEs)

initialUE_Identity:

tmsi_and_LAI: (TMSI_and_LAI_GSM_MAP)

tmsi (TMSI_GSM_MAP):00010001001000100011001101000100

lai:

plmn_Identity:

mcc:

Digit:0
Digit:0
Digit:1

mnc:

Digit:0
Digit:1

lac:0000000000000001

rrc_TransactionIdentifier:0
activationTime: Omit

new_U_RNTI: (U_RNTI)

srnc_Identity:000000000001
s_RNTI:00000000000000000001

new_c_RNTI (C_RNTI): Omit
rrc_StateIndicator:cell_DCH
utran_DRX_CycleLengthCoeff (UTRAN_DRX_CycleLengthCoefficient):9

capabilityUpdateRequirement:

ue_RadioCapabilityFDDUpdateRequirement:true
ue_RadioCapabilityTDDUpdateRequirement:false

systemSpecificCapUpdateReqList:

SystemSpecificCapUpdateReq:gsm

srb_InformationSetupList: (SRB_InformationSetupList2)

SRB_InformationSetup:

rb_Identity: Omit

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_UM_RLC_Mode:

transmissionRLC_Discard: Omit

dl_RLC_Mode:

dl_UM_RLC_Mode:

rb_MappingInfo:

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

dch (TransportChannelIdentity):5

logicalChannelIdentity:1

rlc_SizeList:

configured:

mac_LogicalChannelPriority:1

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

dch (TransportChannelIdentity):10

logicalChannelIdentity:1

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

rach:

logicalChannelIdentity:1

rlc_SizeList:

explicitList: (RLC_SizeExplicitList)

RLC_SizeInfo:

rlc_SizeIndex:1

mac_LogicalChannelPriority:1

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

fach:

logicalChannelIdentity:1

SRB_InformationSetup:

rb_Identity: Omit

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

rb_MappingInfo:

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

dch (TransportChannelIdentity):5

logicalChannelIdentity:2

rlc_SizeList:

configured:

mac_LogicalChannelPriority:2

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

dch (TransportChannelIdentity):10

logicalChannelIdentity:2

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

rach:

logicalChannelIdentity:2

rlc_SizeList:

explicitList: (RLC_SizeExplicitList)

RLC_SizeInfo:

rlc_SizeIndex:1

mac_LogicalChannelPriority:2

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

fach:

logicalChannelIdentity:2

SRB_InformationSetup:

rb_Identity: Omit

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

rb_MappingInfo:

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

dch (TransportChannelIdentity):5

logicalChannelIdentity:3

rlc_SizeList:

configured:

mac_LogicalChannelPriority:3

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

dch (TransportChannelIdentity):10

logicalChannelIdentity:3

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

rach:

logicalChannelIdentity:3

rlc_SizeList:

explicitList: (RLC_SizeExplicitList)

RLC_SizeInfo:

rlc_SizeIndex:1

mac_LogicalChannelPriority:3

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

fach:

logicalChannelIdentity:3

SRB_InformationSetup:

rb_Identity: Omit

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

rb_MappingInfo:

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

dch (TransportChannelIdentity):5

logicalChannelIdentity:4

rlc_SizeList:

configured:

mac_LogicalChannelPriority:4

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

dch (TransportChannelIdentity):10

logicalChannelIdentity:4

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

rach:

logicalChannelIdentity:4

rlc_SizeList:

explicitList: (RLC_SizeExplicitList)

RLC_SizeInfo:

rlc_SizeIndex:1

mac_LogicalChannelPriority:4

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

fach:

logicalChannelIdentity:4

ul_CommonTransChInfo:

tfc_Subset: Omit

prach_TFCS: (TFCS) Omit

modeSpecificInfo:

fdd:

ul_TFCS: (TFCS)

normalTFCI_Signalling: (ExplicitTFCS_Configuration)

complete: (TFCS_ReconfAdd)

ctfcSize:

ctfc2Bit:

:

ctfc2:0

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc2:1

powerOffsetInformation:

gainFactorInformation:

signalledGainFactors:

modeSpecificInfo:

fdd:

gainFactorBetaC (GainFactor):11

gainFactorBetaD (GainFactor):15
referenceTFC_ID:0

powerOffsetPp_m: Omit

ul_AddReconfTransChInfoList:

UL_AddReconfTransChInformation:

ul_TransportChannelType (UL_TrCH_Type):dch
transportChannelIdentity:5

transportFormatSet:

dedicatedTransChTFS:

tti:

tti10: (DedicatedDynamicTF_InfoList)

DedicatedDynamicTF_Info:

rlc_Size:

bitMode: (BitModeRLC_SizeInfo)

sizeType2:

part1:2
part2: Omit

numberOfTbSizeList:

NumberOfTransportBlocks:

zero:

NumberOfTransportBlocks:

one:

logicalChannelList:

allSizes:

semistaticTF_Information:

channelCodingType:

convolutional (CodingRate):third

rateMatchingAttribute:192
crc_Size:crc16

dl_CommonTransChInfo:

sccpch_TFCS: (TFCS) Omit

modeSpecificInfo:

fdd:

dl_Parameters:

sameAsUL:

dl_AddReconfTransChInfoList:

DL_AddReconfTransChInformation:

dl_TransportChannelType (DL_TrCH_Type):dch
dl_transportChannelIdentity (TransportChannelIdentity):10

tfs_SignallingMode:

sameAsULTrCH: (UL_TransportChannelIdentity)

ul_TransportChannelType (UL_TrCH_Type):dch
ul_TransportChannelIdentity (TransportChannelIdentity):5

dch_QualityTarget: (QualityTarget)

bler_QualityValue:-20

dummy: (TM_SignallingInfo) Omit

frequencyInfo: Omit

maxAllowedUL_TX_Power: Omit

ul_ChannelRequirement:

ul_DPCH_Info:

ul_DPCH_PowerControlInfo:

fdd:

dpcch_PowerOffset:-40
pc_Preamble:1
sRB_delay:7

powerControlAlgorithm:

algorithm1 (TPC_StepSizeFDD):0

modeSpecificInfo:

fdd:

scramblingCodeType:longSC
scramblingCode (UL_ScramblingCode):0
numberOfDPDCH: Omit
spreadingFactor:sf64
tfci_Existence:true
numberOfFBI_Bits: Omit
puncturingLimit:pl1

dl_CommonInformation:

dl_DPCH_InfoCommon:

cfnHandling:

initialise:

cfntargetsfnframeoffset: Omit

modeSpecificInfo:

fdd:

dl_DPCH_PowerControlInfo:

modeSpecificInfo:

fdd:

dpc_Mode:singleTPC

powerOffsetPilot_pdpdch:0

dl_rate_matching_restriction: Omit

spreadingFactorAndPilot: (SF512_AndPilot)

sfd128 (PilotBits128):pb4

positionFixedOrFlexible:fixed
tfci_Existence:false

modeSpecificInfo:

fdd:

defaultDPCH_OffsetValue (DefaultDPCH_OffsetValueFDD):0

dpch_CompressedModeInfo: Omit

tx_DiversityMode:noDiversity

ssdt_Information: Omit

dl_InformationPerRL_List:

DL_InformationPerRL:

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode:100

pdsch_SHO_DCH_Info: Omit

pdsch_CodeMapping: Omit

dl_DPCH_InfoPerRL:

fdd:

pCPICH_UsageForChannelEst:mayBeUsed
dpch_FrameOffset:0

secondaryCPICH_Info: Omit

dl_ChannelisationCodeList:

DL_ChannelisationCode:

secondaryScramblingCode:1

sf_AndCodeNumber: (SF512_AndCodeNumber)

sf128:0

scramblingCodeChange:noCodeChange

tpc_CombinationIndex:0
ssdt_CellIdentity: Omit
closedLoopTimingAdjMode: Omit

sccpch_InfoforFACH: Omit

laterNonCriticalExtensions: Omit

specialLI:true

#### PHY_DATA_REQ

MAC PHY @ 00:06:56.490

BTS unit: 1:1
Channel No: 0 Name: FACH
CFN: 186

Message Details:

TFI:2
TB set size:336
TB size:168
TB set (raw, each TB word aligned):

[0]40 25 F8 30 E7 22 24 46
[8]68 80 02 01 00 01 00 04
[16]00 00 4D 82 69 00 40 26
[24]3A 10 10 89 0D 42 00 02
[32]81 9E 8E 46 C9 A6 7C 9C
[40]4E 74 20 00

TB set (decoded):

TB 0:

TCTF:64
MAC SDU (160 bits):

[0]25 F8 30 E7 22 24 46 68
[8]80 02 01 00 01 00 04 00
[16]00 4D 82 69

TB 1:

TCTF:64
MAC SDU (160 bits):

[0]26 3A 10 10 89 0D 42 00
[8]02 81 9E 8E 46 C9 A6 7C
[16]9C 4E 74 20

#### PHY_DATA_REQ

MAC PHY @ 00:06:56.500

BTS unit: 1:1
Channel No: 0 Name: FACH
CFN: 187

Message Details:

TFI:2
TB set size:336
TB size:168
TB set (raw, each TB word aligned):

[0]40 28 A5 12 3A 8C 00 15
[8]13 3D 1C 8D 93 4C F9 38
[16]9C E8 42 52 24 00 40 2A
[24]B5 28 00 4A 46 7A 39 1B
[32]26 99 F2 71 39 D0 86 B4
[40]49 EA 70 00

TB set (decoded):

TB 0:

TCTF:64
MAC SDU (160 bits):

[0]28 A5 12 3A 8C 00 15 13
[8]3D 1C 8D 93 4C F9 38 9C
[16]E8 42 52 24

TB 1:

TCTF:64
MAC SDU (160 bits):

[0]2A B5 28 00 4A 46 7A 39
[8]1B 26 99 F2 71 39 D0 86
[16]B4 49 EA 70

#### PHY_DATA_REQ

MAC PHY @ 00:06:56.510

BTS unit: 1:1
Channel No: 0 Name: FACH
CFN: 188

Message Details:

TFI:2
TB set size:336
TB size:168
TB set (raw, each TB word aligned):

[0]40 2C 00 D4 C8 00 06 25
[8]2B F0 02 00 08 82 23 BF
[16]66 08 98 95 A5 00 40 2F
[24]23 FE 47 82 00 00 01 3F
[32]90 0A 14 00 02 06 40 00
[40]0C 28 08 00

TB set (decoded):

TB 0:

TCTF:64
MAC SDU (160 bits):

[0]2C 00 D4 C8 00 06 25 2B
[8]F0 02 00 08 82 23 BF 66
[16]08 98 95 A5

TB 1:

TCTF:64
MAC SDU (160 bits):

[0]2F 23 FE 47 82 00 00 01
[8]3F 90 0A 14 00 02 06 40
[16]00 0C 28 08

#### CPHY_SYNC_IND

PHY RRC @ 00:06:56.750

BTS unit: 1:1
Channel No: 0 Name: U_DPCH
CFN: 212

Message Details:

#### PHY_DATA_IND

PHY MAC @ 00:06:56.930

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 210

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 00 04 A0 80 00 5A 00
[8]00 59 1A 85 50 6A 4C 26
[16]84 62 C0 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 00 4A 08 00 05 A0 00
[8]05 91 A8 55 06 A4 C2 68
[16]46 2C

#### PHY_DATA_IND

PHY MAC @ 00:06:56.940

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 211

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 00 D1 5F E9 40 20 80
[8]00 80 01 18 A1 40 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 0D 15 FE 94 02 08 00
[8]08 00 11 8A 14 00 00 00
[16]00 00

#### PHY_DATA_REQ

MAC PHY @ 00:06:56.950

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 232

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]10 20 02 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]02 00 20 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### RLC_AM_DATA_IND

LLA RRC @ 00:06:56.960

Channel ID: Rb2
Cell ID: -1

Message Details:

RLC_AM_DATA_IND:

cellId:-1

routingInfo:

rB_Identity:2

integrityResult:

integrityUsed (IntegrityStatus):i_pass

aM_message:

uL_DCCH_Message:

integrityCheckInfo: Omit

message: (UL_DCCH_MessageType)

rrcConnectionSetupComplete:

rrc_TransactionIdentifier:0

startList:

STARTSingle:

cn_DomainIdentity:cs_domain
start_Value:00000000000000010110

STARTSingle:

cn_DomainIdentity:ps_domain
start_Value:00000000000000000010

ue_RadioAccessCapability:

accessStratumReleaseIndicator:r99

pdcp_Capability:

losslessSRNS_RelocationSupport:true

supportForRfc2507:

notSupported:

rlc_Capability:

totalRLC_AM_BufferSize:kb50
maximumRLC_WindowSize:mws2047
maximumAM_EntityNumber (MaximumAM_EntityNumberRLC_Cap):am6

transportChannelCapability:

dl_TransChCapability:

maxNoBitsReceived (MaxNoBits):b6400
maxConvCodeBitsReceived (MaxNoBits):b640

turboDecodingSupport: (TurboSupport)

supported (MaxNoBits):b6400

maxSimultaneousTransChs (MaxSimultaneousTransChsDL):e8
maxSimultaneousCCTrCH_Count:1
maxReceivedTransportBlocks (MaxTransportBlocksDL):tb32
maxNumberOfTFC (MaxNumberOfTFC_DL):tfc128
maxNumberOfTF:tf64

ul_TransChCapability:

maxNoBitsTransmitted (MaxNoBits):b3840
maxConvCodeBitsTransmitted (MaxNoBits):b640

turboEncodingSupport: (TurboSupport)

supported (MaxNoBits):b3840

maxSimultaneousTransChs (MaxSimultaneousTransChsUL):e8

modeSpecificInfo:

fdd:

maxTransmittedBlocks (MaxTransportBlocksUL):tb8
maxNumberOfTFC (MaxNumberOfTFC_UL):tfc32
maxNumberOfTF:tf32

rf_Capability:

fddRF_Capability:

ue_PowerClass:4
txRxFrequencySeparation:mhz190

tddRF_Capability: Omit

physicalChannelCapability:

fddPhysChCapability:

downlinkPhysChCapability: (DL_PhysChCapabilityFDD)

maxNoDPCH_PDSCH_Codes:3
maxNoPhysChBitsReceived:b19200
supportForSF_512:false
supportOfPDSCH:false

simultaneousSCCPCH_DPCH_Reception:

notSupported:

uplinkPhysChCapability: (UL_PhysChCapabilityFDD)

maxNoDPDCH_BitsTransmitted:b2400
supportOfPCPCH:false

tddPhysChCapability: Omit

ue_MultiModeRAT_Capability:

multiRAT_CapabilityList: (MultiRAT_Capability)

supportOfGSM:false
supportOfMulticarrier:false

multiModeCapability:fdd

securityCapability:

cipheringAlgorithmCap:0000000000000001
integrityProtectionAlgorithmCap:0000000000000010

ue_positioning_Capability:

standaloneLocMethodsSupported:false
ue_BasedOTDOA_Supported:false
networkAssistedGPS_Supported:noNetworkAssistedGPS
supportForUE_GPS_TimingOfCellFrames:false
supportForIPDL:false

measurementCapability:

downlinkCompressedMode: (CompressedModeMeasCapability)

fdd_Measurements:true
tdd_Measurements: Omit

gsm_Measurements:

gsm900:false
dcs1800:false
gsm1900:false

multiCarrierMeasurements: Omit

uplinkCompressedMode: (CompressedModeMeasCapability)

fdd_Measurements:true
tdd_Measurements: Omit

gsm_Measurements:

gsm900:false
dcs1800:false
gsm1900:false

multiCarrierMeasurements: Omit

ue_RATSpecificCapability: (InterRAT_UE_RadioAccessCapabilityList) Omit

v370NonCriticalExtensions: Omit

#### PHY_DATA_IND

PHY MAC @ 00:06:57.160

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 233

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 00 D1 5F E9 40 20 80
[8]00 80 01 18 A1 40 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 0D 15 FE 94 02 08 00
[8]08 00 11 8A 14 00 00 00
[16]00 00

#### PHY_DATA_REQ

MAC PHY @ 00:06:57.170

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 254

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]10 20 02 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]02 00 20 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:06:57.190

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 236

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 00 01 58 21 D0 0F 84
[8]04 09 80 78 88 00 00 82
[16]82 A1 60 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 00 15 82 1D 00 F8 40
[8]40 98 07 88 80 00 08 28
[16]2A 16

#### PHY_DATA_IND

PHY MAC @ 00:06:57.200

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 237

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 00 87 00 02 00 0C D5
[8]89 1B 8B 88 0C 02 FA 04
[16]C3 B2 A0 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 08 70 00 20 00 CD 58
[8]91 B8 B8 80 C0 2F A0 4C
[16]3B 2A

#### PHY_DATA_IND

PHY MAC @ 00:06:57.210

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 238

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 01 51 1F E1 98 81 62
[8]80 20 00 04 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 15 11 FE 19 88 16 28
[8]02 00 00 40 00 00 00 00
[16]00 00

#### PHY_DATA_REQ

MAC PHY @ 00:06:57.220

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 3

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 03 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_REQ

MAC PHY @ 00:06:57.250

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 6

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 00 50 FF E1 42 00 61
[8]01 61 C0 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 05 0F FE 14 20 06 10
[8]16 1C 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:06:57.430

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 4

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 01 51 1F E1 98 81 62
[8]80 20 00 04 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 15 11 FE 19 88 16 28
[8]02 00 00 40 00 00 00 00
[16]00 00

#### PHY_DATA_REQ

MAC PHY @ 00:06:57.440

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 25

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 03 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_REQ

MAC PHY @ 00:06:57.450

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 26

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 00 50 FF E1 42 00 61
[8]01 61 C0 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 05 0F FE 14 20 06 10
[8]16 1C 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:06:57.490

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 10

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 01 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 10 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:06:57.710

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 32

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 01 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 10 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### RLC_UM_DATA_REQ

RRC LLA @ 00:06:58.220

Channel ID: Rb1
Cell ID: -1

Message Details:

RLC_UM_DATA_REQ:

cellId:-1

routingInfo:

rB_Identity:1

uM_message:

dL_DCCH_Message:

integrityCheckInfo: Omit

message: (DL_DCCH_MessageType)

rrcConnectionRelease:

r3:

rrcConnectionRelease_r3: (RRCConnectionRelease_r3_IEs)

rrc_TransactionIdentifier:0
n_308:1
releaseCause:normalEvent

rplmn_information: Omit

laterNonCriticalExtensions: Omit

specialLI:false

#### PHY_DATA_REQ

MAC PHY @ 00:06:58.240

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 105

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]00 10 7F E3 C8 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:0
MAC SDU (144 bits):

[0]01 07 FE 3C 80 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:06:58.480

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 109

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]00 10 5F E4 40 00 01 00
[8]80 00 B0 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:0
MAC SDU (144 bits):

[0]01 05 FE 44 00 00 10 08
[8]00 0B 00 00 00 00 00 00
[16]00 00

#### RLC_UM_DATA_IND

LLA RRC @ 00:06:58.490

Channel ID: Rb1
Cell ID: -1

Message Details:

RLC_UM_DATA_IND:

cellId:-1

routingInfo:

rB_Identity:1

integrityResult:

integrityUsed (IntegrityStatus):i_pass

uM_message:

uL_DCCH_Message:

integrityCheckInfo: Omit

message: (UL_DCCH_MessageType)

rrcConnectionReleaseComplete:

rrc_TransactionIdentifier:0

errorIndication: (FailureCauseWithProtErr) Omit

laterNonCriticalExtensions: Omit

#### PHY_DATA_IND

PHY MAC @ 00:06:58.640

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 125

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]00 30 5F E4 40 00 01 00
[8]80 00 B0 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:0
MAC SDU (144 bits):

[0]03 05 FE 44 00 00 10 08
[8]00 0B 00 00 00 00 00 00
[16]00 00

#### RLC_UM_DATA_IND

LLA RRC @ 00:06:58.660

Channel ID: Rb1
Cell ID: -1

Message Details:

RLC_UM_DATA_IND:

cellId:-1

routingInfo:

rB_Identity:1

integrityResult:

integrityUsed (IntegrityStatus):i_pass

uM_message:

uL_DCCH_Message:

integrityCheckInfo: Omit

message: (UL_DCCH_MessageType)

rrcConnectionReleaseComplete:

rrc_TransactionIdentifier:0

errorIndication: (FailureCauseWithProtErr) Omit

laterNonCriticalExtensions: Omit

#### CRLC_Config_REQ

RRC LLA @ 00:06:58.660

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:1

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC_Config_CNF

LLA RRC @ 00:06:58.680

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:1

#### CRLC_Config_REQ

RRC LLA @ 00:06:58.680

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:2

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC_Config_CNF

LLA RRC @ 00:06:58.690

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:2

#### CRLC_Config_REQ

RRC LLA @ 00:06:58.690

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:3

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CPHY_OUTSYNC_IND

PHY RRC @ 00:06:58.690

BTS unit: 1:1
Channel No: 0 Name: U_DPCH
CFN: 150

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:06:58.710

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:3

#### CRLC_Config_REQ

RRC LLA @ 00:06:58.710

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:4

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC_Config_CNF

LLA RRC @ 00:06:58.720

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:4

#### CRLC_Config_REQ

RRC LLA @ 00:06:58.720

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:1

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode)

dl_UM_RLC_Mode:

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):136

dl_RLCModeInfo: (UL_RLC_Mode)

ul_UM_RLC_Mode:

transmissionRLC_Discard:

timerBasedNoExplicit (NoExplicitDiscard):dt100

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity):1
dLlogicalChannelIdentity (LogicalChannelIdentity):1
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC_Config_CNF

LLA RRC @ 00:06:58.740

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:1

#### CRLC_Config_REQ

RRC LLA @ 00:06:58.740

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:2

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode)

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):128

dl_RLCModeInfo: (UL_RLC_Mode)

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity):2
dLlogicalChannelIdentity (LogicalChannelIdentity):2
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC_Config_CNF

LLA RRC @ 00:06:58.750

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:2

#### CRLC_Config_REQ

RRC LLA @ 00:06:58.750

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:3

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode)

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):128

dl_RLCModeInfo: (UL_RLC_Mode)

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity):3
dLlogicalChannelIdentity (LogicalChannelIdentity):3
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC_Config_CNF

LLA RRC @ 00:06:58.770

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:3

#### CRLC_Config_REQ

RRC LLA @ 00:06:58.770

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:4

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode)

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):128

dl_RLCModeInfo: (UL_RLC_Mode)

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity):4
dLlogicalChannelIdentity (LogicalChannelIdentity):4
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC_Config_CNF

LLA RRC @ 00:06:58.790

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:4

#### PHY_DATA_IND

PHY MAC @ 00:11:17.870

BTS unit: 1:1
Channel No: 0 Name: U_RACH
CFN: 192

Message Details:

TFI:0
TB set size:168
TB size:168
TB set (raw):

[0]08 44 48 8C D1 00 04 02
[8]00 02 C0 00 00 00 00 00
[16]00 00 00 00 00 00

TB set (decoded):

TB 0:

TCTF:0
MAC SDU (166 bits):

[0]21 11 22 33 44 00 10 08
[8]00 0B 00 00 00 00 00 00
[16]00 00 00 00 00

#### RLC_TR_DATA_IND

LLA RRC @ 00:11:17.890

Channel ID: Rb0
Cell ID: 0

Message Details:

RLC_TR_DATA_IND:

cellId:0

routingInfo:

rB_Identity:0

tM_message:

uL_CCCH_Message:

integrityCheckInfo: Omit

message: (UL_CCCH_MessageType)

rrcConnectionRequest:

initialUE_Identity:

tmsi_and_LAI: (TMSI_and_LAI_GSM_MAP)

tmsi (TMSI_GSM_MAP):00010001001000100011001101000100

lai:

plmn_Identity:

mcc:

Digit:0
Digit:0
Digit:1

mnc:

Digit:0
Digit:1

lac:0000000000000001

establishmentCause:registration
protocolErrorIndicator:noError

measuredResultsOnRACH: Omit

v3d0NonCriticalExtensions: Omit

#### PHY_DATA_IND

PHY MAC @ 00:11:21.970

BTS unit: 1:1
Channel No: 0 Name: U_RACH
CFN: 90

Message Details:

TFI:0
TB set size:168
TB size:168
TB set (raw):

[0]08 44 48 8C D1 00 04 02
[8]00 02 C0 00 00 00 00 00
[16]00 00 00 00 00 00

TB set (decoded):

TB 0:

TCTF:0
MAC SDU (166 bits):

[0]21 11 22 33 44 00 10 08
[8]00 0B 00 00 00 00 00 00
[16]00 00 00 00 00

#### RLC_TR_DATA_IND

LLA RRC @ 00:11:21.990

Channel ID: Rb0
Cell ID: 0

Message Details:

RLC_TR_DATA_IND:

cellId:0

routingInfo:

rB_Identity:0

tM_message:

uL_CCCH_Message:

integrityCheckInfo: Omit

message: (UL_CCCH_MessageType)

rrcConnectionRequest:

initialUE_Identity:

tmsi_and_LAI: (TMSI_and_LAI_GSM_MAP)

tmsi (TMSI_GSM_MAP):00010001001000100011001101000100

lai:

plmn_Identity:

mcc:

Digit:0
Digit:0
Digit:1

mnc:

Digit:0
Digit:1

lac:0000000000000001

establishmentCause:registration
protocolErrorIndicator:noError

measuredResultsOnRACH: Omit

v3d0NonCriticalExtensions: Omit

#### PHY_DATA_IND

PHY MAC @ 00:11:26.060

BTS unit: 1:1
Channel No: 0 Name: U_RACH
CFN: 243

Message Details:

TFI:0
TB set size:168
TB size:168
TB set (raw):

[0]08 44 48 8C D1 00 04 02
[8]00 02 C0 00 00 00 00 00
[16]00 00 00 00 00 00

TB set (decoded):

TB 0:

TCTF:0
MAC SDU (166 bits):

[0]21 11 22 33 44 00 10 08
[8]00 0B 00 00 00 00 00 00
[16]00 00 00 00 00

#### RLC_TR_DATA_IND

LLA RRC @ 00:11:26.070

Channel ID: Rb0
Cell ID: 0

Message Details:

RLC_TR_DATA_IND:

cellId:0

routingInfo:

rB_Identity:0

tM_message:

uL_CCCH_Message:

integrityCheckInfo: Omit

message: (UL_CCCH_MessageType)

rrcConnectionRequest:

initialUE_Identity:

tmsi_and_LAI: (TMSI_and_LAI_GSM_MAP)

tmsi (TMSI_GSM_MAP):00010001001000100011001101000100

lai:

plmn_Identity:

mcc:

Digit:0
Digit:0
Digit:1

mnc:

Digit:0
Digit:1

lac:0000000000000001

establishmentCause:registration
protocolErrorIndicator:noError

measuredResultsOnRACH: Omit

v3d0NonCriticalExtensions: Omit

#### PHY_DATA_IND

PHY MAC @ 00:11:30.170

BTS unit: 1:1
Channel No: 0 Name: U_RACH
CFN: 142

Message Details:

TFI:0
TB set size:168
TB size:168
TB set (raw):

[0]08 44 48 8C D1 00 04 02
[8]00 02 C0 00 00 00 00 00
[16]00 00 00 00 00 00

TB set (decoded):

TB 0:

TCTF:0
MAC SDU (166 bits):

[0]21 11 22 33 44 00 10 08
[8]00 0B 00 00 00 00 00 00
[16]00 00 00 00 00

#### RLC_TR_DATA_IND

LLA RRC @ 00:11:30.190

Channel ID: Rb0
Cell ID: 0

Message Details:

RLC_TR_DATA_IND:

cellId:0

routingInfo:

rB_Identity:0

tM_message:

uL_CCCH_Message:

integrityCheckInfo: Omit

message: (UL_CCCH_MessageType)

rrcConnectionRequest:

initialUE_Identity:

tmsi_and_LAI: (TMSI_and_LAI_GSM_MAP)

tmsi (TMSI_GSM_MAP):00010001001000100011001101000100

lai:

plmn_Identity:

mcc:

Digit:0
Digit:0
Digit:1

mnc:

Digit:0
Digit:1

lac:0000000000000001

establishmentCause:registration
protocolErrorIndicator:noError

measuredResultsOnRACH: Omit

v3d0NonCriticalExtensions: Omit

#### PHY_DATA_IND

PHY MAC @ 00:11:49.370

BTS unit: 1:1
Channel No: 0 Name: U_RACH
CFN: 14

Message Details:

TFI:0
TB set size:168
TB size:168
TB set (raw):

[0]08 44 48 8C D1 00 04 02
[8]00 02 C0 00 00 00 00 00
[16]00 00 00 00 00 00

TB set (decoded):

TB 0:

TCTF:0
MAC SDU (166 bits):

[0]21 11 22 33 44 00 10 08
[8]00 0B 00 00 00 00 00 00
[16]00 00 00 00 00

#### RLC_TR_DATA_IND

LLA RRC @ 00:11:49.380

Channel ID: Rb0
Cell ID: 0

Message Details:

RLC_TR_DATA_IND:

cellId:0

routingInfo:

rB_Identity:0

tM_message:

uL_CCCH_Message:

integrityCheckInfo: Omit

message: (UL_CCCH_MessageType)

rrcConnectionRequest:

initialUE_Identity:

tmsi_and_LAI: (TMSI_and_LAI_GSM_MAP)

tmsi (TMSI_GSM_MAP):00010001001000100011001101000100

lai:

plmn_Identity:

mcc:

Digit:0
Digit:0
Digit:1

mnc:

Digit:0
Digit:1

lac:0000000000000001

establishmentCause:registration
protocolErrorIndicator:noError

measuredResultsOnRACH: Omit

v3d0NonCriticalExtensions: Omit

#### PHY_DATA_IND

PHY MAC @ 00:11:53.470

BTS unit: 1:1
Channel No: 0 Name: U_RACH
CFN: 168

Message Details:

TFI:0
TB set size:168
TB size:168
TB set (raw):

[0]08 44 48 8C D1 00 04 02
[8]00 02 C0 00 00 00 00 00
[16]00 00 00 00 00 00

TB set (decoded):

TB 0:

TCTF:0
MAC SDU (166 bits):

[0]21 11 22 33 44 00 10 08
[8]00 0B 00 00 00 00 00 00
[16]00 00 00 00 00

#### RLC_TR_DATA_IND

LLA RRC @ 00:11:53.470

Channel ID: Rb0
Cell ID: 0

Message Details:

RLC_TR_DATA_IND:

cellId:0

routingInfo:

rB_Identity:0

tM_message:

uL_CCCH_Message:

integrityCheckInfo: Omit

message: (UL_CCCH_MessageType)

rrcConnectionRequest:

initialUE_Identity:

tmsi_and_LAI: (TMSI_and_LAI_GSM_MAP)

tmsi (TMSI_GSM_MAP):00010001001000100011001101000100

lai:

plmn_Identity:

mcc:

Digit:0
Digit:0
Digit:1

mnc:

Digit:0
Digit:1

lac:0000000000000001

establishmentCause:registration
protocolErrorIndicator:noError

measuredResultsOnRACH: Omit

v3d0NonCriticalExtensions: Omit

#### PHY_DATA_IND

PHY MAC @ 00:11:57.610

BTS unit: 1:1
Channel No: 0 Name: U_RACH
CFN: 70

Message Details:

TFI:0
TB set size:168
TB size:168
TB set (raw):

[0]08 44 48 8C D1 00 04 02
[8]00 02 C0 00 00 00 00 00
[16]00 00 00 00 00 00

TB set (decoded):

TB 0:

TCTF:0
MAC SDU (166 bits):

[0]21 11 22 33 44 00 10 08
[8]00 0B 00 00 00 00 00 00
[16]00 00 00 00 00

#### RLC_TR_DATA_IND

LLA RRC @ 00:11:57.630

Channel ID: Rb0
Cell ID: 0

Message Details:

RLC_TR_DATA_IND:

cellId:0

routingInfo:

rB_Identity:0

tM_message:

uL_CCCH_Message:

integrityCheckInfo: Omit

message: (UL_CCCH_MessageType)

rrcConnectionRequest:

initialUE_Identity:

tmsi_and_LAI: (TMSI_and_LAI_GSM_MAP)

tmsi (TMSI_GSM_MAP):00010001001000100011001101000100

lai:

plmn_Identity:

mcc:

Digit:0
Digit:0
Digit:1

mnc:

Digit:0
Digit:1

lac:0000000000000001

establishmentCause:registration
protocolErrorIndicator:noError

measuredResultsOnRACH: Omit

v3d0NonCriticalExtensions: Omit

#### PHY_DATA_IND

PHY MAC @ 00:12:01.710

BTS unit: 1:1
Channel No: 0 Name: U_RACH
CFN: 224

Message Details:

TFI:0
TB set size:168
TB size:168
TB set (raw):

[0]08 44 48 8C D1 00 04 02
[8]00 02 C0 00 00 00 00 00
[16]00 00 00 00 00 00

TB set (decoded):

TB 0:

TCTF:0
MAC SDU (166 bits):

[0]21 11 22 33 44 00 10 08
[8]00 0B 00 00 00 00 00 00
[16]00 00 00 00 00

#### RLC_TR_DATA_IND

LLA RRC @ 00:12:01.740

Channel ID: Rb0
Cell ID: 0

Message Details:

RLC_TR_DATA_IND:

cellId:0

routingInfo:

rB_Identity:0

tM_message:

uL_CCCH_Message:

integrityCheckInfo: Omit

message: (UL_CCCH_MessageType)

rrcConnectionRequest:

initialUE_Identity:

tmsi_and_LAI: (TMSI_and_LAI_GSM_MAP)

tmsi (TMSI_GSM_MAP):00010001001000100011001101000100

lai:

plmn_Identity:

mcc:

Digit:0
Digit:0
Digit:1

mnc:

Digit:0
Digit:1

lac:0000000000000001

establishmentCause:registration
protocolErrorIndicator:noError

measuredResultsOnRACH: Omit

v3d0NonCriticalExtensions: Omit

#### PHY_DATA_IND

PHY MAC @ 00:12:21.060

BTS unit: 1:1
Channel No: 0 Name: U_RACH
CFN: 111

Message Details:

TFI:0
TB set size:168
TB size:168
TB set (raw):

[0]08 44 48 8C D1 00 04 02
[8]00 02 C0 00 00 00 00 00
[16]00 00 00 00 00 00

TB set (decoded):

TB 0:

TCTF:0
MAC SDU (166 bits):

[0]21 11 22 33 44 00 10 08
[8]00 0B 00 00 00 00 00 00
[16]00 00 00 00 00

#### RLC_TR_DATA_IND

LLA RRC @ 00:12:21.080

Channel ID: Rb0
Cell ID: 0

Message Details:

RLC_TR_DATA_IND:

cellId:0

routingInfo:

rB_Identity:0

tM_message:

uL_CCCH_Message:

integrityCheckInfo: Omit

message: (UL_CCCH_MessageType)

rrcConnectionRequest:

initialUE_Identity:

tmsi_and_LAI: (TMSI_and_LAI_GSM_MAP)

tmsi (TMSI_GSM_MAP):00010001001000100011001101000100

lai:

plmn_Identity:

mcc:

Digit:0
Digit:0
Digit:1

mnc:

Digit:0
Digit:1

lac:0000000000000001

establishmentCause:registration
protocolErrorIndicator:noError

measuredResultsOnRACH: Omit

v3d0NonCriticalExtensions: Omit

#### RLC_UM_DATA_REQ

RRC LLA @ 00:12:22.790

Channel ID: Rb0
Cell ID: 0

Message Details:

RLC_UM_DATA_REQ:

cellId:0

routingInfo:

rB_Identity:0

uM_message:

dL_CCCH_Message:

integrityCheckInfo: Omit

message: (DL_CCCH_MessageType)

rrcConnectionSetup:

r3:

rrcConnectionSetup_r3: (RRCConnectionSetup_r3_IEs)

initialUE_Identity:

tmsi_and_LAI: (TMSI_and_LAI_GSM_MAP)

tmsi (TMSI_GSM_MAP):00010001001000100011001101000100

lai:

plmn_Identity:

mcc:

Digit:0
Digit:0
Digit:1

mnc:

Digit:0
Digit:1

lac:0000000000000001

rrc_TransactionIdentifier:0
activationTime: Omit

new_U_RNTI: (U_RNTI)

srnc_Identity:000000000001
s_RNTI:00000000000000000001

new_c_RNTI (C_RNTI): Omit
rrc_StateIndicator:cell_DCH
utran_DRX_CycleLengthCoeff (UTRAN_DRX_CycleLengthCoefficient):9

capabilityUpdateRequirement:

ue_RadioCapabilityFDDUpdateRequirement:true
ue_RadioCapabilityTDDUpdateRequirement:false

systemSpecificCapUpdateReqList:

SystemSpecificCapUpdateReq:gsm

srb_InformationSetupList: (SRB_InformationSetupList2)

SRB_InformationSetup:

rb_Identity: Omit

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_UM_RLC_Mode:

transmissionRLC_Discard: Omit

dl_RLC_Mode:

dl_UM_RLC_Mode:

rb_MappingInfo:

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

dch (TransportChannelIdentity):5

logicalChannelIdentity:1

rlc_SizeList:

configured:

mac_LogicalChannelPriority:1

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

dch (TransportChannelIdentity):10

logicalChannelIdentity:1

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

rach:

logicalChannelIdentity:1

rlc_SizeList:

explicitList: (RLC_SizeExplicitList)

RLC_SizeInfo:

rlc_SizeIndex:1

mac_LogicalChannelPriority:1

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

fach:

logicalChannelIdentity:1

SRB_InformationSetup:

rb_Identity: Omit

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

rb_MappingInfo:

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

dch (TransportChannelIdentity):5

logicalChannelIdentity:2

rlc_SizeList:

configured:

mac_LogicalChannelPriority:2

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

dch (TransportChannelIdentity):10

logicalChannelIdentity:2

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

rach:

logicalChannelIdentity:2

rlc_SizeList:

explicitList: (RLC_SizeExplicitList)

RLC_SizeInfo:

rlc_SizeIndex:1

mac_LogicalChannelPriority:2

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

fach:

logicalChannelIdentity:2

SRB_InformationSetup:

rb_Identity: Omit

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

rb_MappingInfo:

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

dch (TransportChannelIdentity):5

logicalChannelIdentity:3

rlc_SizeList:

configured:

mac_LogicalChannelPriority:3

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

dch (TransportChannelIdentity):10

logicalChannelIdentity:3

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

rach:

logicalChannelIdentity:3

rlc_SizeList:

explicitList: (RLC_SizeExplicitList)

RLC_SizeInfo:

rlc_SizeIndex:1

mac_LogicalChannelPriority:3

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

fach:

logicalChannelIdentity:3

SRB_InformationSetup:

rb_Identity: Omit

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

rb_MappingInfo:

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

dch (TransportChannelIdentity):5

logicalChannelIdentity:4

rlc_SizeList:

configured:

mac_LogicalChannelPriority:4

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

dch (TransportChannelIdentity):10

logicalChannelIdentity:4

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

rach:

logicalChannelIdentity:4

rlc_SizeList:

explicitList: (RLC_SizeExplicitList)

RLC_SizeInfo:

rlc_SizeIndex:1

mac_LogicalChannelPriority:4

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

fach:

logicalChannelIdentity:4

ul_CommonTransChInfo:

tfc_Subset: Omit

prach_TFCS: (TFCS) Omit

modeSpecificInfo:

fdd:

ul_TFCS: (TFCS)

normalTFCI_Signalling: (ExplicitTFCS_Configuration)

complete: (TFCS_ReconfAdd)

ctfcSize:

ctfc2Bit:

:

ctfc2:0

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc2:1

powerOffsetInformation:

gainFactorInformation:

signalledGainFactors:

modeSpecificInfo:

fdd:

gainFactorBetaC (GainFactor):11

gainFactorBetaD (GainFactor):15
referenceTFC_ID:0

powerOffsetPp_m: Omit

ul_AddReconfTransChInfoList:

UL_AddReconfTransChInformation:

ul_TransportChannelType (UL_TrCH_Type):dch
transportChannelIdentity:5

transportFormatSet:

dedicatedTransChTFS:

tti:

tti10: (DedicatedDynamicTF_InfoList)

DedicatedDynamicTF_Info:

rlc_Size:

bitMode: (BitModeRLC_SizeInfo)

sizeType2:

part1:2
part2: Omit

numberOfTbSizeList:

NumberOfTransportBlocks:

zero:

NumberOfTransportBlocks:

one:

logicalChannelList:

allSizes:

semistaticTF_Information:

channelCodingType:

convolutional (CodingRate):third

rateMatchingAttribute:192
crc_Size:crc16

dl_CommonTransChInfo:

sccpch_TFCS: (TFCS) Omit

modeSpecificInfo:

fdd:

dl_Parameters:

sameAsUL:

dl_AddReconfTransChInfoList:

DL_AddReconfTransChInformation:

dl_TransportChannelType (DL_TrCH_Type):dch
dl_transportChannelIdentity (TransportChannelIdentity):10

tfs_SignallingMode:

sameAsULTrCH: (UL_TransportChannelIdentity)

ul_TransportChannelType (UL_TrCH_Type):dch
ul_TransportChannelIdentity (TransportChannelIdentity):5

dch_QualityTarget: (QualityTarget)

bler_QualityValue:-20

dummy: (TM_SignallingInfo) Omit

frequencyInfo: Omit

maxAllowedUL_TX_Power: Omit

ul_ChannelRequirement:

ul_DPCH_Info:

ul_DPCH_PowerControlInfo:

fdd:

dpcch_PowerOffset:-40
pc_Preamble:1
sRB_delay:7

powerControlAlgorithm:

algorithm1 (TPC_StepSizeFDD):0

modeSpecificInfo:

fdd:

scramblingCodeType:longSC
scramblingCode (UL_ScramblingCode):0
numberOfDPDCH: Omit
spreadingFactor:sf64
tfci_Existence:true
numberOfFBI_Bits: Omit
puncturingLimit:pl1

dl_CommonInformation:

dl_DPCH_InfoCommon:

cfnHandling:

initialise:

cfntargetsfnframeoffset: Omit

modeSpecificInfo:

fdd:

dl_DPCH_PowerControlInfo:

modeSpecificInfo:

fdd:

dpc_Mode:singleTPC

powerOffsetPilot_pdpdch:0

dl_rate_matching_restriction: Omit

spreadingFactorAndPilot: (SF512_AndPilot)

sfd128 (PilotBits128):pb4

positionFixedOrFlexible:fixed
tfci_Existence:false

modeSpecificInfo:

fdd:

defaultDPCH_OffsetValue (DefaultDPCH_OffsetValueFDD):0

dpch_CompressedModeInfo: Omit

tx_DiversityMode:noDiversity

ssdt_Information: Omit

dl_InformationPerRL_List:

DL_InformationPerRL:

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode:100

pdsch_SHO_DCH_Info: Omit

pdsch_CodeMapping: Omit

dl_DPCH_InfoPerRL:

fdd:

pCPICH_UsageForChannelEst:mayBeUsed
dpch_FrameOffset:0

secondaryCPICH_Info: Omit

dl_ChannelisationCodeList:

DL_ChannelisationCode:

secondaryScramblingCode:1

sf_AndCodeNumber: (SF512_AndCodeNumber)

sf128:0

scramblingCodeChange:noCodeChange

tpc_CombinationIndex:0
ssdt_CellIdentity: Omit
closedLoopTimingAdjMode: Omit

sccpch_InfoforFACH: Omit

laterNonCriticalExtensions: Omit

specialLI:true

#### PHY_DATA_REQ

MAC PHY @ 00:12:22.830

BTS unit: 1:1
Channel No: 0 Name: FACH
CFN: 52

Message Details:

TFI:2
TB set size:336
TB size:168
TB set (raw, each TB word aligned):

[0]40 31 F8 30 E7 22 24 46
[8]68 80 02 01 00 01 00 04
[16]00 00 4D 82 69 00 40 32
[24]3A 10 10 89 0D 42 00 02
[32]81 9E 8E 46 C9 A6 7C 9C
[40]4E 74 20 00

TB set (decoded):

TB 0:

TCTF:64
MAC SDU (160 bits):

[0]31 F8 30 E7 22 24 46 68
[8]80 02 01 00 01 00 04 00
[16]00 4D 82 69

TB 1:

TCTF:64
MAC SDU (160 bits):

[0]32 3A 10 10 89 0D 42 00
[8]02 81 9E 8E 46 C9 A6 7C
[16]9C 4E 74 20

#### PHY_DATA_REQ

MAC PHY @ 00:12:22.840

BTS unit: 1:1
Channel No: 0 Name: FACH
CFN: 53

Message Details:

TFI:2
TB set size:336
TB size:168
TB set (raw, each TB word aligned):

[0]40 34 A5 12 3A 8C 00 15
[8]13 3D 1C 8D 93 4C F9 38
[16]9C E8 42 52 24 00 40 36
[24]B5 28 00 4A 46 7A 39 1B
[32]26 99 F2 71 39 D0 86 B4
[40]49 EA 70 00

TB set (decoded):

TB 0:

TCTF:64
MAC SDU (160 bits):

[0]34 A5 12 3A 8C 00 15 13
[8]3D 1C 8D 93 4C F9 38 9C
[16]E8 42 52 24

TB 1:

TCTF:64
MAC SDU (160 bits):

[0]36 B5 28 00 4A 46 7A 39
[8]1B 26 99 F2 71 39 D0 86
[16]B4 49 EA 70

#### PHY_DATA_REQ

MAC PHY @ 00:12:22.850

BTS unit: 1:1
Channel No: 0 Name: FACH
CFN: 54

Message Details:

TFI:2
TB set size:336
TB size:168
TB set (raw, each TB word aligned):

[0]40 38 00 D4 C8 00 06 25
[8]2B F0 02 00 08 82 23 BF
[16]66 08 98 95 A5 00 40 3B
[24]23 FE 47 82 00 00 01 3F
[32]90 0A 14 00 02 06 40 00
[40]0C 28 08 00

TB set (decoded):

TB 0:

TCTF:64
MAC SDU (160 bits):

[0]38 00 D4 C8 00 06 25 2B
[8]F0 02 00 08 82 23 BF 66
[16]08 98 95 A5

TB 1:

TCTF:64
MAC SDU (160 bits):

[0]3B 23 FE 47 82 00 00 01
[8]3F 90 0A 14 00 02 06 40
[16]00 0C 28 08

#### CPHY_SYNC_IND

PHY RRC @ 00:12:23.090

BTS unit: 1:1
Channel No: 0 Name: U_DPCH
CFN: 78

Message Details:

#### PHY_DATA_IND

PHY MAC @ 00:12:23.280

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 77

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 00 04 A0 80 00 5A 00
[8]00 59 1A 85 50 6A 4C 26
[16]84 62 C0 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 00 4A 08 00 05 A0 00
[8]05 91 A8 55 06 A4 C2 68
[16]46 2C

#### PHY_DATA_IND

PHY MAC @ 00:12:23.290

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 78

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 00 D1 5F E9 40 20 80
[8]00 80 01 18 A1 40 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 0D 15 FE 94 02 08 00
[8]08 00 11 8A 14 00 00 00
[16]00 00

#### RLC_AM_DATA_IND

LLA RRC @ 00:12:23.300

Channel ID: Rb2
Cell ID: -1

Message Details:

RLC_AM_DATA_IND:

cellId:-1

routingInfo:

rB_Identity:2

integrityResult:

integrityUsed (IntegrityStatus):i_pass

aM_message:

uL_DCCH_Message:

integrityCheckInfo: Omit

message: (UL_DCCH_MessageType)

rrcConnectionSetupComplete:

rrc_TransactionIdentifier:0

startList:

STARTSingle:

cn_DomainIdentity:cs_domain
start_Value:00000000000000010110

STARTSingle:

cn_DomainIdentity:ps_domain
start_Value:00000000000000000010

ue_RadioAccessCapability:

accessStratumReleaseIndicator:r99

pdcp_Capability:

losslessSRNS_RelocationSupport:true

supportForRfc2507:

notSupported:

rlc_Capability:

totalRLC_AM_BufferSize:kb50
maximumRLC_WindowSize:mws2047
maximumAM_EntityNumber (MaximumAM_EntityNumberRLC_Cap):am6

transportChannelCapability:

dl_TransChCapability:

maxNoBitsReceived (MaxNoBits):b6400
maxConvCodeBitsReceived (MaxNoBits):b640

turboDecodingSupport: (TurboSupport)

supported (MaxNoBits):b6400

maxSimultaneousTransChs (MaxSimultaneousTransChsDL):e8
maxSimultaneousCCTrCH_Count:1
maxReceivedTransportBlocks (MaxTransportBlocksDL):tb32
maxNumberOfTFC (MaxNumberOfTFC_DL):tfc128
maxNumberOfTF:tf64

ul_TransChCapability:

maxNoBitsTransmitted (MaxNoBits):b3840
maxConvCodeBitsTransmitted (MaxNoBits):b640

turboEncodingSupport: (TurboSupport)

supported (MaxNoBits):b3840

maxSimultaneousTransChs (MaxSimultaneousTransChsUL):e8

modeSpecificInfo:

fdd:

maxTransmittedBlocks (MaxTransportBlocksUL):tb8
maxNumberOfTFC (MaxNumberOfTFC_UL):tfc32
maxNumberOfTF:tf32

rf_Capability:

fddRF_Capability:

ue_PowerClass:4
txRxFrequencySeparation:mhz190

tddRF_Capability: Omit

physicalChannelCapability:

fddPhysChCapability:

downlinkPhysChCapability: (DL_PhysChCapabilityFDD)

maxNoDPCH_PDSCH_Codes:3
maxNoPhysChBitsReceived:b19200
supportForSF_512:false
supportOfPDSCH:false

simultaneousSCCPCH_DPCH_Reception:

notSupported:

uplinkPhysChCapability: (UL_PhysChCapabilityFDD)

maxNoDPDCH_BitsTransmitted:b2400
supportOfPCPCH:false

tddPhysChCapability: Omit

ue_MultiModeRAT_Capability:

multiRAT_CapabilityList: (MultiRAT_Capability)

supportOfGSM:false
supportOfMulticarrier:false

multiModeCapability:fdd

securityCapability:

cipheringAlgorithmCap:0000000000000001
integrityProtectionAlgorithmCap:0000000000000010

ue_positioning_Capability:

standaloneLocMethodsSupported:false
ue_BasedOTDOA_Supported:false
networkAssistedGPS_Supported:noNetworkAssistedGPS
supportForUE_GPS_TimingOfCellFrames:false
supportForIPDL:false

measurementCapability:

downlinkCompressedMode: (CompressedModeMeasCapability)

fdd_Measurements:true
tdd_Measurements: Omit

gsm_Measurements:

gsm900:false
dcs1800:false
gsm1900:false

multiCarrierMeasurements: Omit

uplinkCompressedMode: (CompressedModeMeasCapability)

fdd_Measurements:true
tdd_Measurements: Omit

gsm_Measurements:

gsm900:false
dcs1800:false
gsm1900:false

multiCarrierMeasurements: Omit

ue_RATSpecificCapability: (InterRAT_UE_RadioAccessCapabilityList) Omit

v370NonCriticalExtensions: Omit

#### PHY_DATA_REQ

MAC PHY @ 00:12:23.300

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 99

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]10 20 02 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]02 00 20 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:12:23.510

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 100

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 00 D1 5F E9 40 20 80
[8]00 80 01 18 A1 40 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 0D 15 FE 94 02 08 00
[8]08 00 11 8A 14 00 00 00
[16]00 00

#### PHY_DATA_REQ

MAC PHY @ 00:12:23.520

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 121

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]10 20 02 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]02 00 20 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:12:23.540

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 103

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 00 01 50 08 80 09 82
[8]84 00 80 78 88 00 00 A7
[16]82 FA 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 00 15 00 88 00 98 28
[8]40 08 07 88 80 00 0A 78
[16]2F A0

#### PHY_DATA_IND

PHY MAC @ 00:12:23.550

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 104

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 00 D1 9F E8 91 19 A2
[8]19 81 A7 8C 40 20 00 2C
[16]00 20 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 0D 19 FE 89 11 9A 21
[8]98 1A 78 C4 02 00 02 C0
[16]02 00

#### PHY_DATA_REQ

MAC PHY @ 00:12:23.560

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 125

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 02 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 20 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_REQ

MAC PHY @ 00:12:23.600

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 129

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 00 01 40 04 80 A2 40
[8]0A AA AA AA AA AA AA AA
[16]AA AA A0 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 00 14 00 48 0A 24 00
[8]AA AA AA AA AA AA AA AA
[16]AA AA

#### PHY_DATA_REQ

MAC PHY @ 00:12:23.610

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 130

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 00 8A AA AA AA AA AA
[8]A4 02 0C C2 20 06 64 5B
[16]A0 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 08 AA AA AA AA AA AA
[8]40 20 CC 22 00 66 45 BA
[16]00 00

#### PHY_DATA_REQ

MAC PHY @ 00:12:23.620

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 131

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 01 51 1F EA A8 8E EC
[8]C2 20 06 64 40 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 15 11 FE AA 88 EE CC
[8]22 00 66 44 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:12:23.770

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 126

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 00 D1 9F E8 91 19 A2
[8]19 81 A7 8C 40 20 00 2C
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 0D 19 FE 89 11 9A 21
[8]98 1A 78 C4 02 00 02 C0
[16]00 00

#### PHY_DATA_REQ

MAC PHY @ 00:12:23.780

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 147

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 02 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 20 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_REQ

MAC PHY @ 00:12:23.800

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 149

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 01 51 1F EA A8 8E EC
[8]C2 20 06 64 40 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 15 11 FE AA 88 EE CC
[8]22 00 66 44 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:12:23.860

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 135

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 03 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:12:24.060

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 155

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 01 51 E6 C0 05 82 AA
[8]2A A2 3B B3 10 82 08 80
[16]19 91 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 15 1E 6C 00 58 2A A2
[8]AA 23 BB 31 08 20 88 01
[16]99 10

#### CRLC_SecurityMode_Config_REQ

RRC LLA @ 00:12:24.070

Cell ID: -1

Message Details:

CRLC_SecurityMode_Config_REQ:

cellId:-1

rlcSecurityInfo: (SecurityInfo)

cn_DomainIdentity:cs_domain
startValue (START_Value):00000000000000000000
cipheringKey: Omit
integrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
gsmCipheringKey: Omit

#### PHY_DATA_REQ

MAC PHY @ 00:12:24.070

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 176

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 03 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:12:24.080

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 157

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 03 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### CRLC_SecurityMode_Config_CNF

LLA RRC @ 00:12:24.080

Cell ID: -1

Message Details:

CRLC_SecurityMode_Config_CNF:

cellId:-1

#### CRLC_SetRRC_MessageSN_REQ

RRC LLA @ 00:12:24.080

Channel ID: Rb0
Cell ID: 0

Message Details:

CRLC_SetRRC_MessageSN_REQ:

cellId:0

routingInfo:

rB_Identity:0

count_I_LSB_UL (RRC_SequenceNumber): Omit
count_I_LSB_DL (RRC_SequenceNumber):0

#### CRLC_SetRRC_MessageSN_CNF

LLA RRC @ 00:12:24.100

Channel ID: Rb0
Cell ID: 0

Message Details:

CRLC_SetRRC_MessageSN_CNF:

cellId:0

routingInfo:

rB_Identity:0

#### CRLC_SetRRC_MessageSN_REQ

RRC LLA @ 00:12:24.100

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_REQ:

cellId:-1

routingInfo:

rB_Identity:1

count_I_LSB_UL (RRC_SequenceNumber): Omit
count_I_LSB_DL (RRC_SequenceNumber):0

#### CRLC_SetRRC_MessageSN_CNF

LLA RRC @ 00:12:24.110

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_CNF:

cellId:-1

routingInfo:

rB_Identity:1

#### CRLC_SetRRC_MessageSN_REQ

RRC LLA @ 00:12:24.110

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_REQ:

cellId:-1

routingInfo:

rB_Identity:2

count_I_LSB_UL (RRC_SequenceNumber): Omit
count_I_LSB_DL (RRC_SequenceNumber):0

#### CRLC_SetRRC_MessageSN_CNF

LLA RRC @ 00:12:24.130

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_CNF:

cellId:-1

routingInfo:

rB_Identity:2

#### CRLC_SetRRC_MessageSN_REQ

RRC LLA @ 00:12:24.130

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_REQ:

cellId:-1

routingInfo:

rB_Identity:3

count_I_LSB_UL (RRC_SequenceNumber): Omit
count_I_LSB_DL (RRC_SequenceNumber):0

#### CRLC_SetRRC_MessageSN_CNF

LLA RRC @ 00:12:24.140

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_CNF:

cellId:-1

routingInfo:

rB_Identity:3

#### CRLC_SetRRC_MessageSN_REQ

RRC LLA @ 00:12:24.140

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_REQ:

cellId:-1

routingInfo:

rB_Identity:4

count_I_LSB_UL (RRC_SequenceNumber): Omit
count_I_LSB_DL (RRC_SequenceNumber):0

#### CRLC_SetRRC_MessageSN_CNF

LLA RRC @ 00:12:24.160

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_CNF:

cellId:-1

routingInfo:

rB_Identity:4

#### CRLC_Integrity_Activate_REQ

RRC LLA @ 00:12:24.160

Cell ID: -1

Message Details:

CRLC_Integrity_Activate_REQ:

cellId:-1
cn_DomainIdentity:cs_domain

integrityActivationInfo:

integrityProtectionModeInfo:

integrityProtectionModeCommand:

startIntegrityProtection:

integrityProtInitNumber:00001111000011110000111100001111

integrityProtectionAlgorithm:uia1

#### CRLC_Integrity_Activate_CNF

LLA RRC @ 00:12:24.180

Cell ID: -1

Message Details:

CRLC_Integrity_Activate_CNF:

cellId:-1

#### CRLC_Integrity_Activate_REQ

RRC LLA @ 00:12:24.180

Cell ID: -1

Message Details:

CRLC_Integrity_Activate_REQ:

cellId:-1
cn_DomainIdentity:cs_domain

integrityActivationInfo:

ul_IntegProtActivationInfo: (IntegrityProtActivationInfoList)

SS_IntegrityProtActivationTimeInfo:

rb_Identity:2
rrc_MessageSequenceNumber:0

#### CMAC Integrity Check Request

RRC MAC @ 00:12:24.190

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000001
Data:

[0]00 00 00 01
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:1 (RNC to UE)
Message Length (bits):128
Message:

[0]80 00 00 01 04 06 00 00
[8]80 01 41 E1 E1 E1 E0 00

#### CMAC Integrity Check Result

MAC RRC @ 00:12:24.190

Message Details:

Integrity Check Result:

MAC-I:11101100100110000001101010011110
Data:

[0]EC 98 1A 9E

#### CRLC_Integrity_Activate_CNF

LLA RRC @ 00:12:24.190

Cell ID: -1

Message Details:

CRLC_Integrity_Activate_CNF:

cellId:-1

#### RLC_AM_DATA_REQ

RRC LLA @ 00:12:24.190

Channel ID: Rb2
Cell ID: -1

Message Details:

RLC_AM_DATA_REQ:

cellId:-1

routingInfo:

rB_Identity:2

confirmationRequest: (AmConfirmationRequest)

noConfirmationRequest:

aM_message:

dL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode:00000000000000000000000000000000
rrc_MessageSequenceNumber:0

message: (DL_DCCH_MessageType)

securityModeCommand:

r3:

securityModeCommand_r3: (SecurityModeCommand_r3_IEs)

rrc_TransactionIdentifier:0

securityCapability:

cipheringAlgorithmCap:0000000000000001
integrityProtectionAlgorithmCap:0000000000000010

cipheringModeInfo: Omit

integrityProtectionModeInfo:

integrityProtectionModeCommand:

startIntegrityProtection:

integrityProtInitNumber:00001111000011110000111100001111

integrityProtectionAlgorithm:uia1

cn_DomainIdentity:cs_domain

ue_SystemSpecificSecurityCap: (InterRAT_UE_SecurityCapList)

InterRAT_UE_SecurityCapability:

gsm:

gsmSecurityCapability:0000000

laterNonCriticalExtensions: Omit

#### PHY_DATA_REQ

MAC PHY @ 00:12:24.210

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 190

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 00 0F 64 C0 D4 F0 C0
[8]60 00 08 00 14 1E 1E 1E
[16]1E 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 00 F6 4C 0D 4F 0C 06
[8]00 00 80 01 41 E1 E1 E1
[16]E0 00

#### PHY_DATA_REQ

MAC PHY @ 00:12:24.220

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 191

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 00 D0 1F E0 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 0D 01 FE 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:12:24.280

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 177

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 01 51 E6 C0 05 82 AA
[8]2A A2 3B B3 10 82 08 80
[16]19 91 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 15 1E 6C 00 58 2A A2
[8]AA 23 BB 31 08 20 88 01
[16]99 10

#### PHY_DATA_REQ

MAC PHY @ 00:12:24.290

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 198

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 03 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_REQ

MAC PHY @ 00:12:24.410

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 210

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 00 D0 1F E0 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 0D 01 FE 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:12:24.460

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 195

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]10 20 02 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]02 00 20 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:12:24.470

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 196

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 01 51 3F EC 59 1B E7
[8]10 D2 10 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 15 13 FE C5 91 BE 71
[8]0D 21 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_REQ

MAC PHY @ 00:12:24.480

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 217

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]10 20 03 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### CMAC Integrity Check Request

RRC MAC @ 00:12:24.490

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000001
Data:

[0]00 00 00 01
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:0 (UE to RNC)
Message Length (bits):72
Message:

[0]80 00 00 01 05 21 00 00
[8]00

#### CMAC Integrity Check Result

MAC RRC @ 00:12:24.490

Message Details:

Integrity Check Result:

MAC-I:10001011001000110111110011100010
Data:

[0]8B 23 7C E2

#### RLC_AM_DATA_IND

LLA RRC @ 00:12:24.490

Channel ID: Rb2
Cell ID: -1

Message Details:

RLC_AM_DATA_IND:

cellId:-1

routingInfo:

rB_Identity:2

integrityResult:

integrityUsed (IntegrityStatus):i_pass

aM_message:

uL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode:10001011001000110111110011100010
rrc_MessageSequenceNumber:1

message: (UL_DCCH_MessageType)

securityModeComplete:

rrc_TransactionIdentifier:0

ul_IntegProtActivationInfo: (IntegrityProtActivationInfo)

rrc_MessageSequenceNumberList:

RRC_MessageSequenceNumber:0
RRC_MessageSequenceNumber:0
RRC_MessageSequenceNumber:0
RRC_MessageSequenceNumber:0
RRC_MessageSequenceNumber:0

rb_UL_CiphActivationTimeInfo: (RB_ActivationTimeInfoList) Omit

laterNonCriticalExtensions: Omit

#### CRLC_Integrity_Activate_REQ

RRC LLA @ 00:12:24.490

Cell ID: -1

Message Details:

CRLC_Integrity_Activate_REQ:

cellId:-1
cn_DomainIdentity:cs_domain

integrityActivationInfo:

ul_IntegProtActivationInfo: (IntegrityProtActivationInfoList)

SS_IntegrityProtActivationTimeInfo:

rb_Identity:0
rrc_MessageSequenceNumber:0

SS_IntegrityProtActivationTimeInfo:

rb_Identity:1
rrc_MessageSequenceNumber:0

SS_IntegrityProtActivationTimeInfo:

rb_Identity:3
rrc_MessageSequenceNumber:0

SS_IntegrityProtActivationTimeInfo:

rb_Identity:4
rrc_MessageSequenceNumber:0

#### CMAC Integrity Check Request

RRC MAC @ 00:12:24.500

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000001
Data:

[0]00 00 00 01
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:1 (RNC to UE)
Message Length (bits):192
Message:

[0]80 00 00 01 81 40 01 E0
[8]A0 40 1E 22 00 00 22 E0
[16]BE 82 24 46 68 94 34 40

#### CMAC Integrity Check Result

MAC RRC @ 00:12:24.500

Message Details:

Integrity Check Result:

MAC-I:00010011010010000100010001011010
Data:

[0]13 48 44 5A

#### CRLC_Integrity_Activate_CNF

LLA RRC @ 00:12:24.500

Cell ID: -1

Message Details:

CRLC_Integrity_Activate_CNF:

cellId:-1

#### PHY_DATA_REQ

MAC PHY @ 00:12:24.530

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 222

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 01 88 9A 42 22 D0 94
[8]00 1E 0A 04 01 E2 20 00
[16]02 2E 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 18 89 A4 22 2D 09 40
[8]01 E0 A0 40 1E 22 00 00
[16]22 E0

#### PHY_DATA_REQ

MAC PHY @ 00:12:24.540

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 223

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 02 51 1F EB E8 22 44
[8]66 89 43 44 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 25 11 FE BE 82 24 46
[8]68 94 34 40 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:12:24.680

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 217

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]10 20 02 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]02 00 20 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:12:24.690

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 218

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 01 51 3F EC 59 1B E7
[8]10 D2 10 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 15 13 FE C5 91 BE 71
[8]0D 21 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_REQ

MAC PHY @ 00:12:24.700

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 239

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]10 20 03 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_REQ

MAC PHY @ 00:12:24.730

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 242

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 02 51 1F EB E8 22 44
[8]66 89 43 44 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 25 11 FE BE 82 24 46
[8]68 94 34 40 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:12:24.780

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 227

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 05 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 50 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:12:24.790

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 228

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 01 D1 5F EA 4D 81 B8
[8]D8 EC 00 08 2C D8 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 1D 15 FE A4 D8 1B 8D
[8]8E C0 00 82 CD 80 00 00
[16]00 00

#### PHY_DATA_REQ

MAC PHY @ 00:12:24.800

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 249

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 04 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 40 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### CMAC Integrity Check Request

RRC MAC @ 00:12:24.800

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000001
Data:

[0]00 00 00 01
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:0 (UE to RNC)
Message Length (bits):80
Message:

[0]80 00 00 01 86 C0 00 82
[8]CD 80

#### CMAC Integrity Check Result

MAC RRC @ 00:12:24.800

Message Details:

Integrity Check Result:

MAC-I:01001001101100000011011100011011
Data:

[0]49 B0 37 1B

#### PHY_DATA_IND

PHY MAC @ 00:12:25.000

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 249

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 05 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 50 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:12:25.010

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 250

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 01 D1 5F EA 4D 81 B8
[8]D8 EC 00 08 2C D8 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 1D 15 FE A4 D8 1B 8D
[8]8E C0 00 82 CD 80 00 00
[16]00 00

#### PHY_DATA_REQ

MAC PHY @ 00:12:25.020

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 15

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 04 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 40 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### CMAC Integrity Check Request

RRC MAC @ 00:12:25.820

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000001
Data:

[0]00 00 00 01
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:1 (RNC to UE)
Message Length (bits):56
Message:

[0]80 00 00 00 83 C8 00

#### CMAC Integrity Check Result

MAC RRC @ 00:12:25.820

Message Details:

Integrity Check Result:

MAC-I:11101100100111000001011111010011
Data:

[0]EC 9C 17 D3

#### RLC_UM_DATA_REQ

RRC LLA @ 00:12:25.820

Channel ID: Rb1
Cell ID: -1

Message Details:

RLC_UM_DATA_REQ:

cellId:-1

routingInfo:

rB_Identity:1

uM_message:

dL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode:00000000000000000000000000000000
rrc_MessageSequenceNumber:0

message: (DL_DCCH_MessageType)

rrcConnectionRelease:

r3:

rrcConnectionRelease_r3: (RRCConnectionRelease_r3_IEs)

rrc_TransactionIdentifier:0
n_308:1
releaseCause:normalEvent

rplmn_information: Omit

laterNonCriticalExtensions: Omit

specialLI:false

#### PHY_DATA_REQ

MAC PHY @ 00:12:25.840

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 97

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]00 10 FF EF 64 E0 BE 98
[8]BC 80 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:0
MAC SDU (144 bits):

[0]01 0F FE F6 4E 0B E9 8B
[8]C8 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:12:26.080

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 101

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]00 10 DF EF BF 16 16 70
[8]C4 00 B0 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:0
MAC SDU (144 bits):

[0]01 0D FE FB F1 61 67 0C
[8]40 0B 00 00 00 00 00 00
[16]00 00

#### CMAC Integrity Check Request

RRC MAC @ 00:12:26.080

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000001
Data:

[0]00 00 00 01
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:0 (UE to RNC)
Message Length (bits):48
Message:

[0]80 00 00 00 84 40

#### CMAC Integrity Check Result

MAC RRC @ 00:12:26.080

Message Details:

Integrity Check Result:

MAC-I:11110111111000101100001011001110
Data:

[0]F7 E2 C2 CE

#### RLC_UM_DATA_IND

LLA RRC @ 00:12:26.080

Channel ID: Rb1
Cell ID: -1

Message Details:

RLC_UM_DATA_IND:

cellId:-1

routingInfo:

rB_Identity:1

integrityResult:

integrityUsed (IntegrityStatus):i_pass

uM_message:

uL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode:11110111111000101100001011001110
rrc_MessageSequenceNumber:1

message: (UL_DCCH_MessageType)

rrcConnectionReleaseComplete:

rrc_TransactionIdentifier:0

errorIndication: (FailureCauseWithProtErr) Omit

laterNonCriticalExtensions: Omit

#### PHY_DATA_IND

PHY MAC @ 00:12:26.240

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 117

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]00 30 DF ED CD 18 3E 01
[8]44 00 B0 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:0
MAC SDU (144 bits):

[0]03 0D FE DC D1 83 E0 14
[8]40 0B 00 00 00 00 00 00
[16]00 00

#### CMAC Integrity Check Request

RRC MAC @ 00:12:26.250

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000010
Data:

[0]00 00 00 02
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:0 (UE to RNC)
Message Length (bits):48
Message:

[0]80 00 00 00 84 40

#### CMAC Integrity Check Result

MAC RRC @ 00:12:26.250

Message Details:

Integrity Check Result:

MAC-I:10111001101000110000011111000000
Data:

[0]B9 A3 07 C0

#### RLC_UM_DATA_IND

LLA RRC @ 00:12:26.250

Channel ID: Rb1
Cell ID: -1

Message Details:

RLC_UM_DATA_IND:

cellId:-1

routingInfo:

rB_Identity:1

integrityResult:

integrityUsed (IntegrityStatus):i_pass

uM_message:

uL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode:10111001101000110000011111000000
rrc_MessageSequenceNumber:2

message: (UL_DCCH_MessageType)

rrcConnectionReleaseComplete:

rrc_TransactionIdentifier:0

errorIndication: (FailureCauseWithProtErr) Omit

laterNonCriticalExtensions: Omit

#### CRLC_Config_REQ

RRC LLA @ 00:12:26.250

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:1

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC_Config_CNF

LLA RRC @ 00:12:26.270

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:1

#### CRLC_Config_REQ

RRC LLA @ 00:12:26.270

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:2

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC_Config_CNF

LLA RRC @ 00:12:26.290

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:2

#### CRLC_Config_REQ

RRC LLA @ 00:12:26.290

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:3

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CPHY_OUTSYNC_IND

PHY RRC @ 00:12:26.290

BTS unit: 1:1
Channel No: 0 Name: U_DPCH
CFN: 142

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:12:26.300

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:3

#### CRLC_Config_REQ

RRC LLA @ 00:12:26.300

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:4

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC_Config_CNF

LLA RRC @ 00:12:26.320

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:4

#### CRLC_Config_REQ

RRC LLA @ 00:12:26.320

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:1

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode)

dl_UM_RLC_Mode:

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):136

dl_RLCModeInfo: (UL_RLC_Mode)

ul_UM_RLC_Mode:

transmissionRLC_Discard:

timerBasedNoExplicit (NoExplicitDiscard):dt100

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity):1
dLlogicalChannelIdentity (LogicalChannelIdentity):1
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC_Config_CNF

LLA RRC @ 00:12:26.330

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:1

#### CRLC_Config_REQ

RRC LLA @ 00:12:26.330

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:2

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode)

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):128

dl_RLCModeInfo: (UL_RLC_Mode)

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity):2
dLlogicalChannelIdentity (LogicalChannelIdentity):2
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC_Config_CNF

LLA RRC @ 00:12:26.350

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:2

#### CRLC_Config_REQ

RRC LLA @ 00:12:26.350

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:3

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode)

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):128

dl_RLCModeInfo: (UL_RLC_Mode)

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity):3
dLlogicalChannelIdentity (LogicalChannelIdentity):3
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC_Config_CNF

LLA RRC @ 00:12:26.360

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:3

#### CRLC_Config_REQ

RRC LLA @ 00:12:26.360

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:4

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode)

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):128

dl_RLCModeInfo: (UL_RLC_Mode)

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity):4
dLlogicalChannelIdentity (LogicalChannelIdentity):4
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC_Config_CNF

LLA RRC @ 00:12:26.380

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:4

#### MMI_CmdReq

RRC LLA @ 00:12:31.390

Message Details:

MMI_CmdReq:

cmd (IA5String):Please switch off the UE

#### MMI_CmdCnf

LLA RRC @ 00:12:38.220

Message Details:

MMI_CmdCnf:

result:true
resultString (IA5String): Omit

#### PHY_DATA_IND

PHY MAC @ 00:12:42.020

BTS unit: 1:1
Channel No: 0 Name: U_RACH
CFN: 159

Message Details:

TFI:0
TB set size:168
TB size:168
TB set (raw):

[0]08 44 48 8C D1 00 04 02
[8]00 02 D0 00 00 00 00 00
[16]00 00 00 00 00 00

TB set (decoded):

TB 0:

TCTF:0
MAC SDU (166 bits):

[0]21 11 22 33 44 00 10 08
[8]00 0B 40 00 00 00 00 00
[16]00 00 00 00 00

#### RLC_TR_DATA_IND

LLA RRC @ 00:12:42.020

Channel ID: Rb0
Cell ID: 0

Message Details:

RLC_TR_DATA_IND:

cellId:0

routingInfo:

rB_Identity:0

tM_message:

uL_CCCH_Message:

integrityCheckInfo: Omit

message: (UL_CCCH_MessageType)

rrcConnectionRequest:

initialUE_Identity:

tmsi_and_LAI: (TMSI_and_LAI_GSM_MAP)

tmsi (TMSI_GSM_MAP):00010001001000100011001101000100

lai:

plmn_Identity:

mcc:

Digit:0
Digit:0
Digit:1

mnc:

Digit:0
Digit:1

lac:0000000000000001

establishmentCause:detach
protocolErrorIndicator:noError

measuredResultsOnRACH: Omit

v3d0NonCriticalExtensions: Omit

#### RLC_UM_DATA_REQ

RRC LLA @ 00:12:42.020

Channel ID: Rb0
Cell ID: 0

Message Details:

RLC_UM_DATA_REQ:

cellId:0

routingInfo:

rB_Identity:0

uM_message:

dL_CCCH_Message:

integrityCheckInfo: Omit

message: (DL_CCCH_MessageType)

rrcConnectionSetup:

r3:

rrcConnectionSetup_r3: (RRCConnectionSetup_r3_IEs)

initialUE_Identity:

tmsi_and_LAI: (TMSI_and_LAI_GSM_MAP)

tmsi (TMSI_GSM_MAP):00010001001000100011001101000100

lai:

plmn_Identity:

mcc:

Digit:0
Digit:0
Digit:1

mnc:

Digit:0
Digit:1

lac:0000000000000001

rrc_TransactionIdentifier:0
activationTime: Omit

new_U_RNTI: (U_RNTI)

srnc_Identity:000000000001
s_RNTI:00000000000000000001

new_c_RNTI (C_RNTI): Omit
rrc_StateIndicator:cell_DCH
utran_DRX_CycleLengthCoeff (UTRAN_DRX_CycleLengthCoefficient):9

capabilityUpdateRequirement:

ue_RadioCapabilityFDDUpdateRequirement:true
ue_RadioCapabilityTDDUpdateRequirement:false

systemSpecificCapUpdateReqList:

SystemSpecificCapUpdateReq:gsm

srb_InformationSetupList: (SRB_InformationSetupList2)

SRB_InformationSetup:

rb_Identity: Omit

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_UM_RLC_Mode:

transmissionRLC_Discard: Omit

dl_RLC_Mode:

dl_UM_RLC_Mode:

rb_MappingInfo:

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

dch (TransportChannelIdentity):5

logicalChannelIdentity:1

rlc_SizeList:

configured:

mac_LogicalChannelPriority:1

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

dch (TransportChannelIdentity):10

logicalChannelIdentity:1

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

rach:

logicalChannelIdentity:1

rlc_SizeList:

explicitList: (RLC_SizeExplicitList)

RLC_SizeInfo:

rlc_SizeIndex:1

mac_LogicalChannelPriority:1

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

fach:

logicalChannelIdentity:1

SRB_InformationSetup:

rb_Identity: Omit

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

rb_MappingInfo:

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

dch (TransportChannelIdentity):5

logicalChannelIdentity:2

rlc_SizeList:

configured:

mac_LogicalChannelPriority:2

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

dch (TransportChannelIdentity):10

logicalChannelIdentity:2

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

rach:

logicalChannelIdentity:2

rlc_SizeList:

explicitList: (RLC_SizeExplicitList)

RLC_SizeInfo:

rlc_SizeIndex:1

mac_LogicalChannelPriority:2

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

fach:

logicalChannelIdentity:2

SRB_InformationSetup:

rb_Identity: Omit

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

rb_MappingInfo:

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

dch (TransportChannelIdentity):5

logicalChannelIdentity:3

rlc_SizeList:

configured:

mac_LogicalChannelPriority:3

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

dch (TransportChannelIdentity):10

logicalChannelIdentity:3

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

rach:

logicalChannelIdentity:3

rlc_SizeList:

explicitList: (RLC_SizeExplicitList)

RLC_SizeInfo:

rlc_SizeIndex:1

mac_LogicalChannelPriority:3

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

fach:

logicalChannelIdentity:3

SRB_InformationSetup:

rb_Identity: Omit

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

rb_MappingInfo:

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

dch (TransportChannelIdentity):5

logicalChannelIdentity:4

rlc_SizeList:

configured:

mac_LogicalChannelPriority:4

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

dch (TransportChannelIdentity):10

logicalChannelIdentity:4

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

rach:

logicalChannelIdentity:4

rlc_SizeList:

explicitList: (RLC_SizeExplicitList)

RLC_SizeInfo:

rlc_SizeIndex:1

mac_LogicalChannelPriority:4

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

fach:

logicalChannelIdentity:4

ul_CommonTransChInfo:

tfc_Subset: Omit

prach_TFCS: (TFCS) Omit

modeSpecificInfo:

fdd:

ul_TFCS: (TFCS)

normalTFCI_Signalling: (ExplicitTFCS_Configuration)

complete: (TFCS_ReconfAdd)

ctfcSize:

ctfc2Bit:

:

ctfc2:0

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc2:1

powerOffsetInformation:

gainFactorInformation:

signalledGainFactors:

modeSpecificInfo:

fdd:

gainFactorBetaC (GainFactor):11

gainFactorBetaD (GainFactor):15
referenceTFC_ID:0

powerOffsetPp_m: Omit

ul_AddReconfTransChInfoList:

UL_AddReconfTransChInformation:

ul_TransportChannelType (UL_TrCH_Type):dch
transportChannelIdentity:5

transportFormatSet:

dedicatedTransChTFS:

tti:

tti10: (DedicatedDynamicTF_InfoList)

DedicatedDynamicTF_Info:

rlc_Size:

bitMode: (BitModeRLC_SizeInfo)

sizeType2:

part1:2
part2: Omit

numberOfTbSizeList:

NumberOfTransportBlocks:

zero:

NumberOfTransportBlocks:

one:

logicalChannelList:

allSizes:

semistaticTF_Information:

channelCodingType:

convolutional (CodingRate):third

rateMatchingAttribute:192
crc_Size:crc16

dl_CommonTransChInfo:

sccpch_TFCS: (TFCS) Omit

modeSpecificInfo:

fdd:

dl_Parameters:

sameAsUL:

dl_AddReconfTransChInfoList:

DL_AddReconfTransChInformation:

dl_TransportChannelType (DL_TrCH_Type):dch
dl_transportChannelIdentity (TransportChannelIdentity):10

tfs_SignallingMode:

sameAsULTrCH: (UL_TransportChannelIdentity)

ul_TransportChannelType (UL_TrCH_Type):dch
ul_TransportChannelIdentity (TransportChannelIdentity):5

dch_QualityTarget: (QualityTarget)

bler_QualityValue:-20

dummy: (TM_SignallingInfo) Omit

frequencyInfo: Omit

maxAllowedUL_TX_Power: Omit

ul_ChannelRequirement:

ul_DPCH_Info:

ul_DPCH_PowerControlInfo:

fdd:

dpcch_PowerOffset:-40
pc_Preamble:1
sRB_delay:7

powerControlAlgorithm:

algorithm1 (TPC_StepSizeFDD):0

modeSpecificInfo:

fdd:

scramblingCodeType:longSC
scramblingCode (UL_ScramblingCode):0
numberOfDPDCH: Omit
spreadingFactor:sf64
tfci_Existence:true
numberOfFBI_Bits: Omit
puncturingLimit:pl1

dl_CommonInformation:

dl_DPCH_InfoCommon:

cfnHandling:

initialise:

cfntargetsfnframeoffset: Omit

modeSpecificInfo:

fdd:

dl_DPCH_PowerControlInfo:

modeSpecificInfo:

fdd:

dpc_Mode:singleTPC

powerOffsetPilot_pdpdch:0

dl_rate_matching_restriction: Omit

spreadingFactorAndPilot: (SF512_AndPilot)

sfd128 (PilotBits128):pb4

positionFixedOrFlexible:fixed
tfci_Existence:false

modeSpecificInfo:

fdd:

defaultDPCH_OffsetValue (DefaultDPCH_OffsetValueFDD):0

dpch_CompressedModeInfo: Omit

tx_DiversityMode:noDiversity

ssdt_Information: Omit

dl_InformationPerRL_List:

DL_InformationPerRL:

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode:100

pdsch_SHO_DCH_Info: Omit

pdsch_CodeMapping: Omit

dl_DPCH_InfoPerRL:

fdd:

pCPICH_UsageForChannelEst:mayBeUsed
dpch_FrameOffset:0

secondaryCPICH_Info: Omit

dl_ChannelisationCodeList:

DL_ChannelisationCode:

secondaryScramblingCode:1

sf_AndCodeNumber: (SF512_AndCodeNumber)

sf128:0

scramblingCodeChange:noCodeChange

tpc_CombinationIndex:0
ssdt_CellIdentity: Omit
closedLoopTimingAdjMode: Omit

sccpch_InfoforFACH: Omit

laterNonCriticalExtensions: Omit

specialLI:true

#### PHY_DATA_REQ

MAC PHY @ 00:12:42.070

BTS unit: 1:1
Channel No: 0 Name: FACH
CFN: 184

Message Details:

TFI:2
TB set size:336
TB size:168
TB set (raw, each TB word aligned):

[0]40 3D F8 30 E7 22 24 46
[8]68 80 02 01 00 01 00 04
[16]00 00 4D 82 69 00 40 3E
[24]3A 10 10 89 0D 42 00 02
[32]81 9E 8E 46 C9 A6 7C 9C
[40]4E 74 20 00

TB set (decoded):

TB 0:

TCTF:64
MAC SDU (160 bits):

[0]3D F8 30 E7 22 24 46 68
[8]80 02 01 00 01 00 04 00
[16]00 4D 82 69

TB 1:

TCTF:64
MAC SDU (160 bits):

[0]3E 3A 10 10 89 0D 42 00
[8]02 81 9E 8E 46 C9 A6 7C
[16]9C 4E 74 20

#### PHY_DATA_REQ

MAC PHY @ 00:12:42.080

BTS unit: 1:1
Channel No: 0 Name: FACH
CFN: 185

Message Details:

TFI:2
TB set size:336
TB size:168
TB set (raw, each TB word aligned):

[0]40 40 A5 12 3A 8C 00 15
[8]13 3D 1C 8D 93 4C F9 38
[16]9C E8 42 52 24 00 40 42
[24]B5 28 00 4A 46 7A 39 1B
[32]26 99 F2 71 39 D0 86 B4
[40]49 EA 70 00

TB set (decoded):

TB 0:

TCTF:64
MAC SDU (160 bits):

[0]40 A5 12 3A 8C 00 15 13
[8]3D 1C 8D 93 4C F9 38 9C
[16]E8 42 52 24

TB 1:

TCTF:64
MAC SDU (160 bits):

[0]42 B5 28 00 4A 46 7A 39
[8]1B 26 99 F2 71 39 D0 86
[16]B4 49 EA 70

#### PHY_DATA_REQ

MAC PHY @ 00:12:42.090

BTS unit: 1:1
Channel No: 0 Name: FACH
CFN: 186

Message Details:

TFI:2
TB set size:336
TB size:168
TB set (raw, each TB word aligned):

[0]40 44 00 D4 C8 00 06 25
[8]2B F0 02 00 08 82 23 BF
[16]66 08 98 95 A5 00 40 47
[24]23 FE 47 82 00 00 01 3F
[32]90 0A 14 00 02 06 40 00
[40]0C 28 08 00

TB set (decoded):

TB 0:

TCTF:64
MAC SDU (160 bits):

[0]44 00 D4 C8 00 06 25 2B
[8]F0 02 00 08 82 23 BF 66
[16]08 98 95 A5

TB 1:

TCTF:64
MAC SDU (160 bits):

[0]47 23 FE 47 82 00 00 01
[8]3F 90 0A 14 00 02 06 40
[16]00 0C 28 08

#### CPHY_SYNC_IND

PHY RRC @ 00:12:42.330

BTS unit: 1:1
Channel No: 0 Name: U_DPCH
CFN: 210

Message Details:

#### PHY_DATA_IND

PHY MAC @ 00:12:42.520

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 209

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 00 04 A0 80 00 0A 00
[8]00 59 1A 85 50 6A 4C 26
[16]84 62 C0 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 00 4A 08 00 00 A0 00
[8]05 91 A8 55 06 A4 C2 68
[16]46 2C

#### PHY_DATA_IND

PHY MAC @ 00:12:42.530

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 210

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 00 D1 5F E9 40 20 80
[8]00 80 01 18 A1 40 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 0D 15 FE 94 02 08 00
[8]08 00 11 8A 14 00 00 00
[16]00 00

#### PHY_DATA_REQ

MAC PHY @ 00:12:42.540

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 231

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]10 20 02 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]02 00 20 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### RLC_AM_DATA_IND

LLA RRC @ 00:12:42.550

Channel ID: Rb2
Cell ID: -1

Message Details:

RLC_AM_DATA_IND:

cellId:-1

routingInfo:

rB_Identity:2

integrityResult:

integrityUsed (IntegrityStatus):i_pass

aM_message:

uL_DCCH_Message:

integrityCheckInfo: Omit

message: (UL_DCCH_MessageType)

rrcConnectionSetupComplete:

rrc_TransactionIdentifier:0

startList:

STARTSingle:

cn_DomainIdentity:cs_domain
start_Value:00000000000000000010

STARTSingle:

cn_DomainIdentity:ps_domain
start_Value:00000000000000000010

ue_RadioAccessCapability:

accessStratumReleaseIndicator:r99

pdcp_Capability:

losslessSRNS_RelocationSupport:true

supportForRfc2507:

notSupported:

rlc_Capability:

totalRLC_AM_BufferSize:kb50
maximumRLC_WindowSize:mws2047
maximumAM_EntityNumber (MaximumAM_EntityNumberRLC_Cap):am6

transportChannelCapability:

dl_TransChCapability:

maxNoBitsReceived (MaxNoBits):b6400
maxConvCodeBitsReceived (MaxNoBits):b640

turboDecodingSupport: (TurboSupport)

supported (MaxNoBits):b6400

maxSimultaneousTransChs (MaxSimultaneousTransChsDL):e8
maxSimultaneousCCTrCH_Count:1
maxReceivedTransportBlocks (MaxTransportBlocksDL):tb32
maxNumberOfTFC (MaxNumberOfTFC_DL):tfc128
maxNumberOfTF:tf64

ul_TransChCapability:

maxNoBitsTransmitted (MaxNoBits):b3840
maxConvCodeBitsTransmitted (MaxNoBits):b640

turboEncodingSupport: (TurboSupport)

supported (MaxNoBits):b3840

maxSimultaneousTransChs (MaxSimultaneousTransChsUL):e8

modeSpecificInfo:

fdd:

maxTransmittedBlocks (MaxTransportBlocksUL):tb8
maxNumberOfTFC (MaxNumberOfTFC_UL):tfc32
maxNumberOfTF:tf32

rf_Capability:

fddRF_Capability:

ue_PowerClass:4
txRxFrequencySeparation:mhz190

tddRF_Capability: Omit

physicalChannelCapability:

fddPhysChCapability:

downlinkPhysChCapability: (DL_PhysChCapabilityFDD)

maxNoDPCH_PDSCH_Codes:3
maxNoPhysChBitsReceived:b19200
supportForSF_512:false
supportOfPDSCH:false

simultaneousSCCPCH_DPCH_Reception:

notSupported:

uplinkPhysChCapability: (UL_PhysChCapabilityFDD)

maxNoDPDCH_BitsTransmitted:b2400
supportOfPCPCH:false

tddPhysChCapability: Omit

ue_MultiModeRAT_Capability:

multiRAT_CapabilityList: (MultiRAT_Capability)

supportOfGSM:false
supportOfMulticarrier:false

multiModeCapability:fdd

securityCapability:

cipheringAlgorithmCap:0000000000000001
integrityProtectionAlgorithmCap:0000000000000010

ue_positioning_Capability:

standaloneLocMethodsSupported:false
ue_BasedOTDOA_Supported:false
networkAssistedGPS_Supported:noNetworkAssistedGPS
supportForUE_GPS_TimingOfCellFrames:false
supportForIPDL:false

measurementCapability:

downlinkCompressedMode: (CompressedModeMeasCapability)

fdd_Measurements:true
tdd_Measurements: Omit

gsm_Measurements:

gsm900:false
dcs1800:false
gsm1900:false

multiCarrierMeasurements: Omit

uplinkCompressedMode: (CompressedModeMeasCapability)

fdd_Measurements:true
tdd_Measurements: Omit

gsm_Measurements:

gsm900:false
dcs1800:false
gsm1900:false

multiCarrierMeasurements: Omit

ue_RATSpecificCapability: (InterRAT_UE_RadioAccessCapabilityList) Omit

v370NonCriticalExtensions: Omit

#### PHY_DATA_IND

PHY MAC @ 00:12:42.750

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 232

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 00 D1 5F E9 40 20 80
[8]00 80 01 18 A1 40 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 0D 15 FE 94 02 08 00
[8]08 00 11 8A 14 00 00 00
[16]00 00

#### PHY_DATA_REQ

MAC PHY @ 00:12:42.760

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 253

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]10 20 02 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]02 00 20 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:12:42.780

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 235

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 00 01 50 08 80 04 02
[8]80 A7 82 FA 08 91 19 A2
[16]20 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 00 15 00 88 00 40 28
[8]0A 78 2F A0 89 11 9A 22
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:12:42.790

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 236

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 00 D0 3F E4 0F 6F 71
[8]E0 EC 80 08 40 18 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 0D 03 FE 40 F6 F7 1E
[8]0E C8 00 84 01 80 00 00
[16]00 00

#### PHY_DATA_REQ

MAC PHY @ 00:12:42.800

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 1

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 02 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 20 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:12:43.010

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 2

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 00 D0 3F E4 00 0F 84
[8]04 09 80 78 88 00 00 82
[16]82 A1 60 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 0D 03 FE 40 00 F8 40
[8]40 98 07 88 80 00 08 28
[16]2A 16

#### PHY_DATA_REQ

MAC PHY @ 00:12:43.020

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 23

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 02 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 20 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### RLC_UM_DATA_REQ

RRC LLA @ 00:12:43.830

Channel ID: Rb1
Cell ID: -1

Message Details:

RLC_UM_DATA_REQ:

cellId:-1

routingInfo:

rB_Identity:1

uM_message:

dL_DCCH_Message:

integrityCheckInfo: Omit

message: (DL_DCCH_MessageType)

rrcConnectionRelease:

r3:

rrcConnectionRelease_r3: (RRCConnectionRelease_r3_IEs)

rrc_TransactionIdentifier:0
n_308:1
releaseCause:normalEvent

rplmn_information: Omit

laterNonCriticalExtensions: Omit

specialLI:false

#### PHY_DATA_REQ

MAC PHY @ 00:12:43.850

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 106

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]00 10 7F E3 C8 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:0
MAC SDU (144 bits):

[0]01 07 FE 3C 80 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:12:44.090

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 110

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]00 10 5F E4 40 00 01 00
[8]80 00 B4 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:0
MAC SDU (144 bits):

[0]01 05 FE 44 00 00 10 08
[8]00 0B 40 00 00 00 00 00
[16]00 00

#### RLC_UM_DATA_IND

LLA RRC @ 00:12:44.100

Channel ID: Rb1
Cell ID: -1

Message Details:

RLC_UM_DATA_IND:

cellId:-1

routingInfo:

rB_Identity:1

integrityResult:

integrityUsed (IntegrityStatus):i_pass

uM_message:

uL_DCCH_Message:

integrityCheckInfo: Omit

message: (UL_DCCH_MessageType)

rrcConnectionReleaseComplete:

rrc_TransactionIdentifier:0

errorIndication: (FailureCauseWithProtErr) Omit

laterNonCriticalExtensions: Omit

#### PHY_DATA_IND

PHY MAC @ 00:12:44.250

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 126

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]00 30 5F E4 40 00 01 00
[8]80 00 B4 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:0
MAC SDU (144 bits):

[0]03 05 FE 44 00 00 10 08
[8]00 0B 40 00 00 00 00 00
[16]00 00

#### RLC_UM_DATA_IND

LLA RRC @ 00:12:44.270

Channel ID: Rb1
Cell ID: -1

Message Details:

RLC_UM_DATA_IND:

cellId:-1

routingInfo:

rB_Identity:1

integrityResult:

integrityUsed (IntegrityStatus):i_pass

uM_message:

uL_DCCH_Message:

integrityCheckInfo: Omit

message: (UL_DCCH_MessageType)

rrcConnectionReleaseComplete:

rrc_TransactionIdentifier:0

errorIndication: (FailureCauseWithProtErr) Omit

laterNonCriticalExtensions: Omit

#### CRLC_Config_REQ

RRC LLA @ 00:12:44.270

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:1

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC_Config_CNF

LLA RRC @ 00:12:44.290

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:1

#### CRLC_Config_REQ

RRC LLA @ 00:12:44.290

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:2

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC_Config_CNF

LLA RRC @ 00:12:44.300

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:2

#### CRLC_Config_REQ

RRC LLA @ 00:12:44.300

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:3

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CPHY_OUTSYNC_IND

PHY RRC @ 00:12:44.300

BTS unit: 1:1
Channel No: 0 Name: U_DPCH
CFN: 151

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:12:44.320

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:3

#### CRLC_Config_REQ

RRC LLA @ 00:12:44.320

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:4

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC_Config_CNF

LLA RRC @ 00:12:44.330

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:4

#### CRLC_Config_REQ

RRC LLA @ 00:12:44.330

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:1

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode)

dl_UM_RLC_Mode:

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):136

dl_RLCModeInfo: (UL_RLC_Mode)

ul_UM_RLC_Mode:

transmissionRLC_Discard:

timerBasedNoExplicit (NoExplicitDiscard):dt100

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity):1
dLlogicalChannelIdentity (LogicalChannelIdentity):1
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC_Config_CNF

LLA RRC @ 00:12:44.350

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:1

#### CRLC_Config_REQ

RRC LLA @ 00:12:44.350

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:2

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode)

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):128

dl_RLCModeInfo: (UL_RLC_Mode)

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity):2
dLlogicalChannelIdentity (LogicalChannelIdentity):2
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC_Config_CNF

LLA RRC @ 00:12:44.360

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:2

#### CRLC_Config_REQ

RRC LLA @ 00:12:44.360

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:3

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode)

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):128

dl_RLCModeInfo: (UL_RLC_Mode)

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity):3
dLlogicalChannelIdentity (LogicalChannelIdentity):3
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC_Config_CNF

LLA RRC @ 00:12:44.410

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:3

#### CRLC_Config_REQ

RRC LLA @ 00:12:44.410

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:4

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode)

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):128

dl_RLCModeInfo: (UL_RLC_Mode)

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity):4
dLlogicalChannelIdentity (LogicalChannelIdentity):4
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC_Config_CNF

LLA RRC @ 00:12:44.430

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:4

#### CRLC_Config_REQ

RRC LLA @ 00:12:46.430

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:1

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC_Config_CNF

LLA RRC @ 00:12:46.440

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:1

#### CRLC_Config_REQ

RRC LLA @ 00:12:46.440

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:2

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC_Config_CNF

LLA RRC @ 00:12:46.460

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:2

#### CRLC_Config_REQ

RRC LLA @ 00:12:46.460

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:3

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC_Config_CNF

LLA RRC @ 00:12:46.470

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:3

#### CRLC_Config_REQ

RRC LLA @ 00:12:46.470

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:4

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC_Config_CNF

LLA RRC @ 00:12:46.490

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:4

#### CMAC_Config_REQ

RRC LLA @ 00:12:46.490

Channel ID: DL-DPCH#1
Cell ID: -1

Message Details:

CMAC_Config_REQ:

cellId:-1

routingInfo:

physicalChannelIdentity:26

ratType:fdd

configMessage:

release:

#### CMAC_Config_CNF

LLA RRC @ 00:12:46.500

Channel ID: DL-DPCH#1
Cell ID: -1

Message Details:

CMAC_Config_CNF:

cellId:-1

routingInfo:

physicalChannelIdentity:26

#### CMAC_Config_REQ

RRC LLA @ 00:12:46.500

Channel ID: UL-DPCH#1
Cell ID: -1

Message Details:

CMAC_Config_REQ:

cellId:-1

routingInfo:

physicalChannelIdentity:20

ratType:fdd

configMessage:

release:

#### CMAC Configuration REQ

LLA MAC @ 00:12:46.510

BTS unit: 1:1
Channel No: 0 Name: D_DPCH
CFN: 116

Message Details:

Configuration Parameters:

Number Of Transport Channels:0
Active Flag:0

Transport Format Combination Set:

Number Of Transport Format Combinations:0

#### CMAC Configuration CNF

MAC LLA @ 00:12:46.510

BTS unit: 1:1
Channel No: 0 Name: D_DPCH
CFN: 116

Message Details:

#### CMAC Configuration REQ

LLA MAC @ 00:12:46.530

BTS unit: 1:1
Channel No: 0 Name: U_DPCH
CFN: 118

Message Details:

Configuration Parameters:

Number Of Transport Channels:0
Active Flag:0

Transport Format Combination Set:

Number Of Transport Format Combinations:0

#### CMAC Configuration CNF

MAC LLA @ 00:12:46.530

BTS unit: 1:1
Channel No: 0 Name: U_DPCH
CFN: 118

Message Details:

#### CMAC_Config_CNF

LLA RRC @ 00:12:46.540

Channel ID: UL-DPCH#1
Cell ID: -1

Message Details:

CMAC_Config_CNF:

cellId:-1

routingInfo:

physicalChannelIdentity:20

#### CPHY_TrCH_Release_REQ

RRC LLA @ 00:12:46.540

Channel ID: DL-DPCH#1
Cell ID: 0

Message Details:

CPHY_TrCH_Release_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:26

trchConfigType:

dch:normal

#### CPHY_TrCH_Release_CNF

LLA RRC @ 00:12:46.550

Channel ID: DL-DPCH#1
Cell ID: 0

Message Details:

CPHY_TrCH_Release_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:26

#### CPHY Transport Channel Release REQ

LLA PHY @ 00:12:46.550

BTS unit: 1:1
Channel No: 0 Name: D_DPCH
CFN: 120

Message Details:

#### CPHY Transport Channel Release CNF

PHY LLA @ 00:12:46.550

BTS unit: 1:1
Channel No: 0 Name: D_DPCH
CFN: 120

Message Details:

#### CPHY_TrCH_Release_REQ

RRC LLA @ 00:12:46.800

Channel ID: UL-DPCH#1
Cell ID: 0

Message Details:

CPHY_TrCH_Release_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:20

trchConfigType:

dch:normal

#### CPHY Transport Channel Release REQ

LLA PHY @ 00:12:46.820

BTS unit: 1:1
Channel No: 0 Name: U_DPCH
CFN: 147

Message Details:

#### CPHY Transport Channel Release CNF

PHY LLA @ 00:12:46.820

BTS unit: 1:1
Channel No: 0 Name: U_DPCH
CFN: 147

Message Details:

#### CPHY_TrCH_Release_CNF

LLA RRC @ 00:12:46.830

Channel ID: UL-DPCH#1
Cell ID: 0

Message Details:

CPHY_TrCH_Release_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:20

#### CPHY_RL_Release_REQ

RRC LLA @ 00:12:46.830

Channel ID: DL-DPCH#1
Cell ID: 0

Message Details:

CPHY_RL_Release_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:26

#### CPHY_RL_Release_CNF

LLA RRC @ 00:12:46.850

Channel ID: DL-DPCH#1
Cell ID: 0

Message Details:

CPHY_RL_Release_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:26

#### CPHY_RL_Release_REQ

RRC LLA @ 00:12:46.850

Channel ID: UL-DPCH#1
Cell ID: 0

Message Details:

CPHY_RL_Release_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:20

#### CPHY Radio Link Release REQ

LLA PHY @ 00:12:46.850

BTS unit: 1:1
Channel No: 0 Name: D_DPCH
CFN: 150

Message Details:

#### CPHY Radio Link Release CNF

PHY LLA @ 00:12:46.850

BTS unit: 1:1
Channel No: 0 Name: D_DPCH
CFN: 150

Message Details:

#### CPHY_RL_Release_CNF

LLA RRC @ 00:12:46.860

Channel ID: UL-DPCH#1
Cell ID: 0

Message Details:

CPHY_RL_Release_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:20

#### CRLC_Config_REQ

RRC LLA @ 00:12:46.860

Channel ID: Rb0
Cell ID: 0

Message Details:

CRLC_Config_REQ:

cellId:0

routingInfo:

rB_Identity:0

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CPHY Radio Link Release REQ

LLA PHY @ 00:12:46.860

BTS unit: 1:1
Channel No: 0 Name: U_DPCH
CFN: 151

Message Details:

#### CPHY Radio Link Release CNF

PHY LLA @ 00:12:46.860

BTS unit: 1:1
Channel No: 0 Name: U_DPCH
CFN: 151

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:12:46.880

Channel ID: Rb0
Cell ID: 0

Message Details:

CRLC_Config_CNF:

cellId:0

routingInfo:

rB_Identity:0

#### CMAC_Config_REQ

RRC LLA @ 00:12:46.880

Channel ID: PRACH#1
Cell ID: 0

Message Details:

CMAC_Config_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:8

ratType:fdd

configMessage:

release:

#### CMAC_Config_CNF

LLA RRC @ 00:12:46.890

Channel ID: PRACH#1
Cell ID: 0

Message Details:

CMAC_Config_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:8

#### CPHY_TrCH_Release_REQ

RRC LLA @ 00:12:46.890

Channel ID: PRACH#1
Cell ID: 0

Message Details:

CPHY_TrCH_Release_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:8

trchConfigType:

nonDch:

#### CMAC Configuration REQ

LLA MAC @ 00:12:46.900

BTS unit: 1:1
Channel No: 0 Name: PRACH
CFN: 155

Message Details:

Configuration Parameters:

Number Of Transport Channels:0
Active Flag:0

Transport Format Combination Set:

Number Of Transport Format Combinations:0

#### CMAC Configuration CNF

MAC LLA @ 00:12:46.900

BTS unit: 1:1
Channel No: 0 Name: PRACH
CFN: 155

Message Details:

#### CPHY_TrCH_Release_CNF

LLA RRC @ 00:12:46.910

Channel ID: PRACH#1
Cell ID: 0

Message Details:

CPHY_TrCH_Release_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:8

#### CPHY_RL_Release_REQ

RRC LLA @ 00:12:46.910

Channel ID: AICH#1
Cell ID: 0

Message Details:

CPHY_RL_Release_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:7

#### CPHY Transport Channel Release REQ

LLA PHY @ 00:12:46.910

BTS unit: 1:1
Channel No: 0 Name: PRACH
CFN: 156

Message Details:

#### CPHY Transport Channel Release CNF

PHY LLA @ 00:12:46.910

BTS unit: 1:1
Channel No: 0 Name: PRACH
CFN: 156

Message Details:

#### CPHY_RL_Release_CNF

LLA RRC @ 00:12:46.930

Channel ID: AICH#1
Cell ID: 0

Message Details:

CPHY_RL_Release_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:7

#### CPHY_RL_Release_REQ

RRC LLA @ 00:12:46.930

Channel ID: PRACH#1
Cell ID: 0

Message Details:

CPHY_RL_Release_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:8

#### CPHY Radio Link Release REQ

LLA PHY @ 00:12:46.930

BTS unit: 1:1
Channel No: 0 Name: AICH
CFN: 158

Message Details:

#### CPHY Radio Link Release CNF

PHY LLA @ 00:12:46.930

BTS unit: 1:1
Channel No: 0 Name: AICH
CFN: 158

Message Details:

#### CPHY_RL_Release_CNF

LLA RRC @ 00:12:46.940

Channel ID: PRACH#1
Cell ID: 0

Message Details:

CPHY_RL_Release_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:8

#### CRLC_Config_REQ

RRC LLA @ 00:12:46.940

Channel ID: RbPcch
Cell ID: 0

Message Details:

CRLC_Config_REQ:

cellId:0

routingInfo:

rB_Identity:-2

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CPHY Radio Link Release REQ

LLA PHY @ 00:12:46.940

BTS unit: 1:1
Channel No: 0 Name: PRACH
CFN: 159

Message Details:

#### CPHY Radio Link Release CNF

PHY LLA @ 00:12:46.940

BTS unit: 1:1
Channel No: 0 Name: PRACH
CFN: 159

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:12:46.960

Channel ID: RbPcch
Cell ID: 0

Message Details:

CRLC_Config_CNF:

cellId:0

routingInfo:

rB_Identity:-2

#### CMAC_Config_REQ

RRC LLA @ 00:12:46.960

Channel ID: S-CCPCH#1
Cell ID: 0

Message Details:

CMAC_Config_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:5

ratType:fdd

configMessage:

release:

#### CMAC Configuration REQ

LLA MAC @ 00:12:46.980

BTS unit: 1:1
Channel No: 0 Name: S_CCPCH
CFN: 163

Message Details:

Configuration Parameters:

Number Of Transport Channels:0
Active Flag:0

Transport Format Combination Set:

Number Of Transport Format Combinations:0

#### CMAC Configuration CNF

MAC LLA @ 00:12:46.980

BTS unit: 1:1
Channel No: 0 Name: S_CCPCH
CFN: 163

Message Details:

#### CMAC_Config_CNF

LLA RRC @ 00:12:46.990

Channel ID: S-CCPCH#1
Cell ID: 0

Message Details:

CMAC_Config_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:5

#### CPHY_TrCH_Release_REQ

RRC LLA @ 00:12:46.990

Channel ID: S-CCPCH#1
Cell ID: 0

Message Details:

CPHY_TrCH_Release_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:5

trchConfigType:

nonDch:

#### CPHY Transport Channel Release REQ

LLA PHY @ 00:12:47.010

BTS unit: 1:1
Channel No: 0 Name: S_CCPCH
CFN: 166

Message Details:

#### CPHY Transport Channel Release CNF

PHY LLA @ 00:12:47.010

BTS unit: 1:1
Channel No: 0 Name: S_CCPCH
CFN: 166

Message Details:

#### CPHY_TrCH_Release_CNF

LLA RRC @ 00:12:47.020

Channel ID: S-CCPCH#1
Cell ID: 0

Message Details:

CPHY_TrCH_Release_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:5

#### CPHY_RL_Release_REQ

RRC LLA @ 00:12:47.020

Channel ID: PICH#1
Cell ID: 0

Message Details:

CPHY_RL_Release_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:6

#### CPHY_RL_Release_CNF

LLA RRC @ 00:12:47.040

Channel ID: PICH#1
Cell ID: 0

Message Details:

CPHY_RL_Release_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:6

#### CPHY_RL_Release_REQ

RRC LLA @ 00:12:47.040

Channel ID: S-CCPCH#1
Cell ID: 0

Message Details:

CPHY_RL_Release_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:5

#### CPHY Radio Link Release REQ

LLA PHY @ 00:12:47.040

BTS unit: 1:1
Channel No: 0 Name: PICH
CFN: 169

Message Details:

#### CPHY Radio Link Release CNF

PHY LLA @ 00:12:47.040

BTS unit: 1:1
Channel No: 0 Name: PICH
CFN: 169

Message Details:

#### CPHY_RL_Release_CNF

LLA RRC @ 00:12:47.050

Channel ID: S-CCPCH#1
Cell ID: 0

Message Details:

CPHY_RL_Release_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:5

#### CRLC_Config_REQ

RRC LLA @ 00:12:47.050

Channel ID: RbBcch
Cell ID: 0

Message Details:

CRLC_Config_REQ:

cellId:0

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CPHY Radio Link Release REQ

LLA PHY @ 00:12:47.050

BTS unit: 1:1
Channel No: 0 Name: S_CCPCH
CFN: 170

Message Details:

#### CPHY Radio Link Release CNF

PHY LLA @ 00:12:47.050

BTS unit: 1:1
Channel No: 0 Name: S_CCPCH
CFN: 170

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:12:47.070

Channel ID: RbBcch
Cell ID: 0

Message Details:

CRLC_Config_CNF:

cellId:0

routingInfo:

rB_Identity:-1

#### CMAC_Config_REQ

RRC LLA @ 00:12:47.070

Channel ID: P-CCPCH
Cell ID: 0

Message Details:

CMAC_Config_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:4

ratType:fdd

configMessage:

release:

#### CMAC Configuration REQ

LLA MAC @ 00:12:47.090

BTS unit: 1:1
Channel No: 0 Name: P_CCPCH
CFN: 174

Message Details:

Configuration Parameters:

Number Of Transport Channels:0
Active Flag:0

Transport Format Combination Set:

Number Of Transport Format Combinations:0

#### CMAC Configuration CNF

MAC LLA @ 00:12:47.090

BTS unit: 1:1
Channel No: 0 Name: P_CCPCH
CFN: 174

Message Details:

#### CMAC_Config_CNF

LLA RRC @ 00:12:47.100

Channel ID: P-CCPCH
Cell ID: 0

Message Details:

CMAC_Config_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:4

#### CPHY_TrCH_Release_REQ

RRC LLA @ 00:12:47.100

Channel ID: P-CCPCH
Cell ID: 0

Message Details:

CPHY_TrCH_Release_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:4

trchConfigType:

nonDch:

#### CPHY_TrCH_Release_CNF

LLA RRC @ 00:12:47.110

Channel ID: P-CCPCH
Cell ID: 0

Message Details:

CPHY_TrCH_Release_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:4

#### CPHY_RL_Release_REQ

RRC LLA @ 00:12:47.110

Channel ID: S-SCH
Cell ID: 0

Message Details:

CPHY_RL_Release_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:2

#### CPHY Transport Channel Release REQ

LLA PHY @ 00:12:47.110

BTS unit: 1:1
Channel No: 0 Name: P_CCPCH
CFN: 176

Message Details:

#### CPHY Transport Channel Release CNF

PHY LLA @ 00:12:47.110

BTS unit: 1:1
Channel No: 0 Name: P_CCPCH
CFN: 176

Message Details:

#### CPHY_RL_Release_CNF

LLA RRC @ 00:12:47.130

Channel ID: S-SCH
Cell ID: 0

Message Details:

CPHY_RL_Release_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:2

#### CPHY_RL_Release_REQ

RRC LLA @ 00:12:47.130

Channel ID: P-SCH
Cell ID: 0

Message Details:

CPHY_RL_Release_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:1

#### CPHY Radio Link Release REQ

LLA PHY @ 00:12:47.130

BTS unit: 1:1
Channel No: 0 Name: S_SCH
CFN: 178

Message Details:

#### CPHY Radio Link Release CNF

PHY LLA @ 00:12:47.130

BTS unit: 1:1
Channel No: 0 Name: S_SCH
CFN: 178

Message Details:

#### CPHY_RL_Release_CNF

LLA RRC @ 00:12:47.140

Channel ID: P-SCH
Cell ID: 0

Message Details:

CPHY_RL_Release_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:1

#### CPHY_RL_Release_REQ

RRC LLA @ 00:12:47.140

Channel ID: P-CCPCH
Cell ID: 0

Message Details:

CPHY_RL_Release_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:4

#### CPHY Radio Link Release REQ

LLA PHY @ 00:12:47.150

BTS unit: 1:1
Channel No: 0 Name: P_SCH
CFN: 180

Message Details:

#### CPHY Radio Link Release CNF

PHY LLA @ 00:12:47.150

BTS unit: 1:1
Channel No: 0 Name: P_SCH
CFN: 180

Message Details:

#### CPHY_RL_Release_CNF

LLA RRC @ 00:12:47.160

Channel ID: P-CCPCH
Cell ID: 0

Message Details:

CPHY_RL_Release_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:4

#### CPHY_RL_Release_REQ

RRC LLA @ 00:12:47.160

Channel ID: P-CPICH
Cell ID: 0

Message Details:

CPHY_RL_Release_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:0

#### CPHY Radio Link Release REQ

LLA PHY @ 00:12:47.160

BTS unit: 1:1
Channel No: 0 Name: P_CCPCH
CFN: 181

Message Details:

#### CPHY Radio Link Release CNF

PHY LLA @ 00:12:47.160

BTS unit: 1:1
Channel No: 0 Name: P_CCPCH
CFN: 181

Message Details:

#### CPHY_RL_Release_CNF

LLA RRC @ 00:12:47.180

Channel ID: P-CPICH
Cell ID: 0

Message Details:

CPHY_RL_Release_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:0

#### CPHY Radio Link Release REQ

LLA PHY @ 00:12:47.180

BTS unit: 1:1
Channel No: 0 Name: P_CPICH
CFN: 183

Message Details:

#### CPHY Radio Link Release CNF

PHY LLA @ 00:12:47.180

BTS unit: 1:1
Channel No: 0 Name: P_CPICH
CFN: 183

Message Details:

#### CGEN Stop REQ

RRC PHY @ 00:12:48.220

Message Details:

#### CGEN Stop CNF

PHY RRC @ 00:12:48.220

Message Details: