- No.: 2
- Timestamp: 17:10:33:325_0
- RFN: 104
- Chip: 21248
- Event: Start Timer
- Source: tc_12_4_1_4c2 LINE 1
- Message Structure:
no details available
- Constraint:
t_Guard (900 Sec)
- BinaryMessage:

- No.: 60
- Timestamp: 17:10:33:333_0
- RFN: 105
- Chip: 14848
- Event: Send
- PCO: Ut
- Message: MMI_CmdReq
- Source: ts_MMI_SetOpModeA LINE 1
- Message Structure:
MMI_CmdReq < Exp>
. (IA5StringType)cmd = -1 <"Please set UE in operation mode A (to support simulataneous CS and PS services>
- Constraint:
ca_MMI_CmdReq
- BinaryMessage:
50 6c 65 61 73 65 20 73 65 74 20 55 45 20 69 6e 20 6f 70 65 72 61 74 69 6f 6e 20 6d 6f 64 65 20 41 20 28 74 6f 20 73 75 70 70 6f 72 74 20 73 69 6d 75 6c 61 74 61 6e 65 6f 75 73 20 43 53 20 61 6e 64 20 50 53 20 73 65 72 76 69 63 65 73 29 20

- No.: 64
- Timestamp: 17:10:36:768_0
- RFN: 448
- Chip: 33792
- Event: Receive
- PCO: Ut
- Message: MMI_CmdCnf
- Source: ts_MMI_SetOpModeA LINE 2
- Message Structure:
MMI_CmdCnf
. (BooleanType)result = TRUE
. (IA5StringType)resultString[0] = ""
- Constraint:
ca_MMI_CmdCnf
- BinaryMessage:
80

- No.: 108
- Timestamp: 17:10:36:773_3
- RFN: 449
- Chip: 16640
- Event: Send
- PCO: Ut
- Message: MMI_CmdReq
- Source: ts_MMI_UE_SwitchOff LINE 2
- Message Structure:
MMI_CmdReq
. (IA5StringType)cmd[-1] = "Please switch off the UE"
- Constraint:
ca_MMI_CmdReq
- BinaryMessage:
50 6c 65 61 73 65 20 73 77 69 74 63 68 20 6f 66 66 20 20 74 68 65 20 55 45

- No.: 112
- Timestamp: 17:11:00:861_0
- RFN: 2858
- Chip: 16128
- Event: Receive
- PCO: Ut
- Message: MMI_CmdCnf
- Source: ts_MMI_UE_SwitchOff LINE 3
- Message Structure:
MMI_CmdCnf
. (BooleanType)result = TRUE
. (IA5StringType)resultString[0] = ""
- Constraint:
ca_MMI_CmdCnf
- BinaryMessage:
80

- No.: 117
- Timestamp: 17:11:00:862_1
- RFN: 2858
- Chip: 19968
- Event: Send
- PCO: CPHY
- Message: CPHY_Ini_REQ
- Source: ts_SS_CellCfg:lt_CelllsAlreadyStarted LINE 5
- Message Structure:
CPHY_Ini_REQ
. (CPHY_Ini_REQ)CPHY_Ini_REQ[-1] = 0
- Constraint:
cas_InitReqDef
- BinaryMessage:
0a 01 00

- No.: 118
- Timestamp: 17:11:00:862_2
- RFN: 2858
- Chip: 21248
- Event: Receive
- PCO: CPHY
- Message: CPHY_Ini_CNF
- Source: ts_SS_CellCfg:lt_CelllsAlreadyStarted LINE 6
- Message Structure:
CPHY_Ini_CNF
- Constraint:
car_IniCnf
- BinaryMessage:
30 02 05 00

- No.: 122
- Timestamp: 17:11:00:864_0
- RFN: 2858
- Chip: 26368
- Event: Send
- PCO: CPHY
- Message: CPHY_Cell_Config_REQ
- Source: ts_SS_CellCfg LINE 6
- Message Structure:
CPHY_Cell_Config_REQ
. (IntegerType)cellId[-1] = 0
. (IntegerType)tcell[-1] = 0
. (IntegerType)sfnOffset[-1] = 0
. FrequencyInfo
. . modeSpecificInfo
. . . FrequencyInfoFDD
. . . . (IntegerType)uarfcn_UL[-1] = 9263
. . . . (IntegerType)uarfcn_DL[-1] = 9663
. (IntegerType)primaryScramblingCode_SS[-1] = 100
. CellTxPowerLevel
. (IntegerType)dLTxAttenuationLevel[-1] = 0
- Constraint:
ca_CellCfgReq
- BinaryMessage:
30 1d 02 01 00 02 01 00 02 01 00 30 0a 30 08 02 02 24 2f 02 02 25 bf 02 01 64 05 00 02 01 00

- No.: 129
- Timestamp: 17:11:01:248_0
- RFN: 2897
- Chip: 4352
- Event: Receive
- PCO: CPHY
- Message: CPHY_Cell_Config_CNF
- Source: ts_SS_CellCfg LINE 7
- Message Structure:
CPHY_Cell_Config_CNF
. (IntegerType)cellId[0] = 0
- Constraint:
ca_CellCfgCnf
- BinaryMessage:
30 03 02 01 00

- No.: 141
- Timestamp: 17:11:01:250_0
- RFN: 2897
- Chip: 14080
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 3
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 0
. (RatType)ratType[0] = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . PrimaryCPICHInfo
. . . . (IntegerType)dl_TxPower_PCPICH[-1] = -60
. . . . (BooleanType)txdiversityIndicator = FALSE
- Constraint:
ca_pCPICH_Info
- BinaryMessage:
30 13 02 01 00 02 01 00 0a 01 00 30 08 30 06 02 01 c4 01 01 00

- No.: 145
- Timestamp: 17:11:01:256_0
- RFN: 2897
- Chip: 35584
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 4
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 0
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 00

- No.: 146
- Timestamp: 17:11:01:257_0
- RFN: 2898
- Chip: 1024
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 5
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 1
. (RatType)ratType[0] = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . PrimarySCHInfo
. . . . (BooleanType)tstdIndicator = FALSE
. . . . (IntegerType)dl_TxPower[-1] = -5
- Constraint:
ca_pSCH_Info
- BinaryMessage:
30 13 02 01 00 02 01 01 0a 01 00 30 08 30 06 01 01 00 02 01 fb

- No.: 150
- Timestamp: 17:11:01:261_0
- RFN: 2898
- Chip: 15360
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 6
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 1
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 01

- No.: 151
- Timestamp: 17:11:01:262_0
- RFN: 2898
- Chip: 19456
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 7
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 2
. (RatType)ratType[0] = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . SecondarySCHInfo
. . . . (BooleanType)tstdIndicator = FALSE
. . . . (IntegerType)dl_TxPower[-1] = -5
- Constraint:
ca_sSCH_Info
- BinaryMessage:
30 13 02 01 00 02 01 02 0a 01 00 30 08 30 06 01 01 00 02 01 fb

- No.: 155
- Timestamp: 17:11:01:400_0
- RFN: 2912
- Chip: 12288
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 8
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 2
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 02

- No.: 156
- Timestamp: 17:11:01:401_0
- RFN: 2912
- Chip: 16640
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 9
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 4
. (RatType)ratType[0] = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . PrimaryCCPCHInfo
. . . . (BooleanType)sttd_Indicator = FALSE
. . . . (IntegerType)dl_TxPower[-1] = -2
- Constraint:
ca_pCCPCH_Info
- BinaryMessage:
30 13 02 01 00 02 01 04 0a 01 00 30 08 30 06 01 01 00 02 01 fe

- No.: 160
- Timestamp: 17:11:01:408_0
- RFN: 2913
- Chip: 4608
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 10
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 4
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 04

- No.: 161
- Timestamp: 17:11:01:411_0
- RFN: 2913
- Chip: 16128
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Config_REQ
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 11
- Message Structure:
CPHY_TrCH_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 4
. (RatType)ratType[0] = 0
. TrChConfigType
. CphyTrchConfigReq
. . SS_ActivationTime
. . ulconnectedTrCHList
. . TFCS
. . dlconnectedTrCHList
. . . CphyTrchConfigReq_setseq_1
. . . . (IntegerType)trchid[-1] = 11
. . . . (SS_DL_TransportChannelType)dl_TransportChannelType[0] = 2
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size[-1] = 246
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional[0] = 0
. . . . . . (IntegerType)rateMatchingAttribute[-1] = 1
. . . . . . (CRC_Size)crc_Size[0] = 3
. . TFCS
. . . ExplicitTFCS_Configuration
. . . . TFCS_ReconfAdd
. . . . . ctfcSize
. . . . . . ctfc2Bit
. . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . (IntegerType)ctfc2[-1] = 0
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . fdd
. . . . . . . . . . . . . (IntegerType)gainFactorBetaC[-1] = 11
. . . . . . . . . . . (IntegerType)gainFactorBetaD[-1] = 15
. . . . . . . . . . . (IntegerType)referenceTFC_ID[-1] = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
- Constraint:
ca_BCH_InfoActNow
- BinaryMessage:
30 4c 02 01 00 02 01 04 0a 01 00 05 00 30 3f 05 00 30 23 30 21 02 01 0b 0a 01 02 30 19 30 0c 30 0a 02 02 00 f6 30 02 05 00 05 00 30 09 0a 01 00 02 01 01 0a 01 03 30 16 30 14 30 12 02 01 00 30 0d 30 0b 30 03 02 01 0b 02 01 0f 02 01 00

- No.: 165
- Timestamp: 17:11:01:418_0
- RFN: 2914
- Chip: 5120
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Config_CNF
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 12
- Message Structure:
CPHY_TrCH_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 4
- Constraint:
ca_TrChCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 04

- No.: 166
- Timestamp: 17:11:01:423_0
- RFN: 2914
- Chip: 22272
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 13
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 4
. (RatType)ratType[0] = 0
. configMessage
. . CmacConfigReq
. . . SS_ActivationTime
. . . UE_Info
. . . . U_RNTI
. . . . (BitStringType)c_RNTI[16] = -
. . . TrCHInfo
. . . . ulconnectedTrCHList
. . . . TFCS
. . . . dlconnectedTrCHList
. . . . . TrCHInfo_setseq_1
. . . . . . (IntegerType)trchid[-1] = 11
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size[-1] = 246
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional[0] = 0
. . . . . . . . (IntegerType)rateMatchingAttribute[-1] = 1
. . . . . . . . (CRC_Size)crc_Size[0] = 3
. . . . TFCS
. . . . . ExplicitTFCS_Configuration
. . . . . . TFCS_ReconfAdd
. . . . . . . ctfcSize
. . . . . . . . ctfc2Bit
. . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . (IntegerType)ctfc2[-1] = 0
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC[-1] = 11
. . . . . . . . . . . . . (IntegerType)gainFactorBetaD[-1] = 15
. . . . . . . . . . . . . (IntegerType)referenceTFC_ID[-1] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . TrCH_LogCHMappingList1
. . . . ulconnectedTrCHList
. . . . dlconnectedTrCHList
. . . . . TrCH_LogCHMappingList1_setseq_1
. . . . . . (IntegerType)trchid[-1] = 11
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation[0] = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType[0] = 2
. . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . . . (LogicalChannelType)logicalChannelType[0] = 0
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 1
. . . . . . . . (IntegerType)rB_Identity[-1] = -1
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_CMAC_CfgInfo
- BinaryMessage:
30 6e 02 01 00 02 01 04 0a 01 00 30 63 05 00 30 00 30 3a 30 20 30 1e 02 01 0b 30 19 30 0c 30 0a 02 02 00 f6 30 02 05 00 05 00 30 09 0a 01 00 02 01 01 0a 01 03 30 16 30 14 30 12 02 01 00 30 0d 30 0b 30 03 02 01 0b 02 01 0f 02 01 00 30 21 30 1f 30 1d 02 01 0b 30 18 30 16 30 11 0a 01 00 0a 01 02 02 01 01 0a 01 00 05 00 02 01 01 02 01 ff

- No.: 170
- Timestamp: 17:11:01:428_0
- RFN: 2915
- Chip: 3584
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 14
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 4
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 04

- No.: 178
- Timestamp: 17:11:01:430_0
- RFN: 2915
- Chip: 10496
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_PCH_FACH_CCCH_Cfg LINE 3
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 5
. (RatType)ratType[0] = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . SecondaryCCPCHInfo
. . . . (IntegerType)scramblingCode[-1] = 0
. . . . SF256_AndCodeNumber
. . . . . (IntegerType)sf64[-1] = 1
. . . . (IntegerType)sCCPCHSlotFormat[-1] = 8
. . . . (IntegerType)timingOffset[-1] = 0
. . . . (PositionFixedOrFlexible)positionFixedOrFlexible[0] = 1
. . . . (BooleanType)sttd_Indicator = FALSE
. . . . (IntegerType)dl_TxPower[-1] = -2
. . . . (IntegerType)powerOffsetOfTFCI_PO1[-1] = 6
. . . . (IntegerType)powerOffsetOfPILOT_PO3[-1] = 6
- Constraint:
ca_sCCPCH_Info
- BinaryMessage:
30 28 02 01 00 02 01 05 0a 01 00 30 1d 30 1b 02 01 00 02 01 01 02 01 08 02 01 00 0a 01 01 01 01 00 02 01 fe 02 01 06 02 01 06

- No.: 182
- Timestamp: 17:11:01:435_0
- RFN: 2915
- Chip: 31232
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_PCH_FACH_CCCH_Cfg LINE 4
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 5
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 05

- No.: 183
- Timestamp: 17:11:01:440_0
- RFN: 2916
- Chip: 12800
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Config_REQ
- Source: ts_SS_PCH_FACH_CCCH_Cfg LINE 5
- Message Structure:
CPHY_TrCH_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 5
. (RatType)ratType[0] = 0
. TrChConfigType
. CphyTrchConfigReq
. . SS_ActivationTime
. . ulconnectedTrCHList
. . TFCS
. . dlconnectedTrCHList
. . . CphyTrchConfigReq_setseq_1
. . . . (IntegerType)trchid[-1] = 12
. . . . (SS_DL_TransportChannelType)dl_TransportChannelType[0] = 3
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size[-1] = 240
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional[0] = 0
. . . . . . (IntegerType)rateMatchingAttribute[-1] = 230
. . . . . . (CRC_Size)crc_Size[0] = 3
. . . CphyTrchConfigReq_setseq_1
. . . . (IntegerType)trchid[-1] = 13
. . . . (SS_DL_TransportChannelType)dl_TransportChannelType[0] = 1
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size[-1] = 168
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . (IntegerType)small[-1] = 2
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional[0] = 0
. . . . . . (IntegerType)rateMatchingAttribute[-1] = 220
. . . . . . (CRC_Size)crc_Size[0] = 3
. . . CphyTrchConfigReq_setseq_1
. . . . (IntegerType)trchid[-1] = 14
. . . . (SS_DL_TransportChannelType)dl_TransportChannelType[0] = 1
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size[-1] = 360
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . (IntegerType)rateMatchingAttribute[-1] = 130
. . . . . . (CRC_Size)crc_Size[0] = 3
. . TFCS
. . . ExplicitTFCS_Configuration
. . . . TFCS_ReconfAdd
. . . . . ctfcSize
. . . . . . ctfc4Bit
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4[-1] = 0
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4[-1] = 1
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4[-1] = 2
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4[-1] = 3
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4[-1] = 4
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4[-1] = 5
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4[-1] = 6
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4[-1] = 8
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . fdd
. . . . . . . . . . . . . (IntegerType)gainFactorBetaC[-1] = 11
. . . . . . . . . . . (IntegerType)gainFactorBetaD[-1] = 15
. . . . . . . . . . . (IntegerType)referenceTFC_ID[-1] = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
- Constraint:
ca_PCH_2_FACH_InfoActNow
- BinaryMessage:
30 81 e4 02 01 00 02 01 05 0a 01 00 05 00 30 81 d6 05 00 30 74 30 24 02 01 0c 0a 01 03 30 1c 30 0e 30 0c 02 02 00 f0 30 04 05 00 05 00 05 00 30 0a 0a 01 00 02 02 00 e6 0a 01 03 30 27 02 01 0d 0a 01 01 30 1f 30 11 30 0f 02 02 00 a8 30 07 05 00 05 00 02 01 02 05 00 30 0a 0a 01 00 02 02 00 dc 0a 01 03 30 23 02 01 0e 0a 01 01 30 1b 30 0e 30 0c 02 02 01 68 30 04 05 00 05 00 05 00 30 09 05 00 02 02 00 82 0a 01 03 30 5c 30 5a 30 08 02 01 00 30 03 02 01 00 30 08 02 01 01 30 03 02 01 00 30 08 02 01 02 30 03 02 01 00 30 08 02 01 03 30 03 02 01 00 30 08 02 01 04 30 03 02 01 00 30 08 02 01 05 30 03 02 01 00 30 08 02 01 06 30 03 02 01 00 30 12 02 01 08 30 0d 30 0b 30 03 02 01 0b 02 01 0f 02 01 00

- No.: 187
- Timestamp: 17:11:01:452_0
- RFN: 2917
- Chip: 21248
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Config_CNF
- Source: ts_SS_PCH_FACH_CCCH_Cfg LINE 6
- Message Structure:
CPHY_TrCH_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 5
- Constraint:
ca_TrChCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 05

- No.: 188
- Timestamp: 17:11:01:460_0
- RFN: 2918
- Chip: 12544
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_SS_PCH_FACH_CCCH_Cfg LINE 7
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 5
. (RatType)ratType[0] = 0
. configMessage
. . CmacConfigReq
. . . SS_ActivationTime
. . . UE_Info
. . . . U_RNTI
. . . . (BitStringType)c_RNTI[16] = -
. . . TrCHInfo
. . . . ulconnectedTrCHList
. . . . TFCS
. . . . dlconnectedTrCHList
. . . . . TrCHInfo_setseq_1
. . . . . . (IntegerType)trchid[-1] = 12
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size[-1] = 240
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional[0] = 0
. . . . . . . . (IntegerType)rateMatchingAttribute[-1] = 230
. . . . . . . . (CRC_Size)crc_Size[0] = 3
. . . . . TrCHInfo_setseq_1
. . . . . . (IntegerType)trchid[-1] = 13
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size[-1] = 168
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . (IntegerType)small[-1] = 2
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional[0] = 0
. . . . . . . . (IntegerType)rateMatchingAttribute[-1] = 220
. . . . . . . . (CRC_Size)crc_Size[0] = 3
. . . . . TrCHInfo_setseq_1
. . . . . . (IntegerType)trchid[-1] = 14
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size[-1] = 360
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . (IntegerType)rateMatchingAttribute[-1] = 130
. . . . . . . . (CRC_Size)crc_Size[0] = 3
. . . . TFCS
. . . . . ExplicitTFCS_Configuration
. . . . . . TFCS_ReconfAdd
. . . . . . . ctfcSize
. . . . . . . . ctfc4Bit
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4[-1] = 0
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4[-1] = 1
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4[-1] = 2
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4[-1] = 3
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4[-1] = 4
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4[-1] = 5
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4[-1] = 6
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4[-1] = 8
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC[-1] = 11
. . . . . . . . . . . . . (IntegerType)gainFactorBetaD[-1] = 15
. . . . . . . . . . . . . (IntegerType)referenceTFC_ID[-1] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . TrCH_LogCHMappingList1
. . . . ulconnectedTrCHList
. . . . dlconnectedTrCHList
. . . . . TrCH_LogCHMappingList1_setseq_1
. . . . . . (IntegerType)trchid[-1] = 12
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation[0] = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType[0] = 3
. . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . . . (LogicalChannelType)logicalChannelType[0] = 1
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 1
. . . . . . . . (IntegerType)rB_Identity[-1] = -2
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
. . . . . TrCH_LogCHMappingList1_setseq_1
. . . . . . (IntegerType)trchid[-1] = 13
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation[0] = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType[0] = 1
. . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 5
. . . . . . . . . . (LogicalChannelType)logicalChannelType[0] = 2
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 1
. . . . . . . . (IntegerType)rB_Identity[-1] = 0
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_CMAC_CfgInfo
- BinaryMessage:
30 82 01 21 02 01 00 02 01 05 0a 01 00 30 82 01 14 05 00 30 00 30 81 cb 30 6b 30 21 02 01 0c 30 1c 30 0e 30 0c 02 02 00 f0 30 04 05 00 05 00 05 00 30 0a 0a 01 00 02 02 00 e6 0a 01 03 30 24 02 01 0d 30 1f 30 11 30 0f 02 02 00 a8 30 07 05 00 05 00 02 01 02 05 00 30 0a 0a 01 00 02 02 00 dc 0a 01 03 30 20 02 01 0e 30 1b 30 0e 30 0c 02 02 01 68 30 04 05 00 05 00 05 00 30 09 05 00 02 02 00 82 0a 01 03 30 5c 30 5a 30 08 02 01 00 30 03 02 01 00 30 08 02 01 01 30 03 02 01 00 30 08 02 01 02 30 03 02 01 00 30 08 02 01 03 30 03 02 01 00 30 08 02 01 04 30 03 02 01 00 30 08 02 01 05 30 03 02 01 00 30 08 02 01 06 30 03 02 01 00 30 12 02 01 08 30 0d 30 0b 30 03 02 01 0b 02 01 0f 02 01 00 30 40 30 3e 30 1d 02 01 0c 30 18 30 16 30 11 0a 01 00 0a 01 03 02 01 01 0a 01 01 05 00 02 01 01 02 01 fe 30 1d 02 01 0d 30 18 30 16 30 11 0a 01 00 0a 01 01 02 01 05 0a 01 02 05 00 02 01 01 02 01 00

- No.: 192
- Timestamp: 17:11:01:467_0
- RFN: 2919
- Chip: 1280
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_SS_PCH_FACH_CCCH_Cfg LINE 8
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 5
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 05

- No.: 193
- Timestamp: 17:11:01:468_0
- RFN: 2919
- Chip: 4608
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_PCH_FACH_CCCH_Cfg LINE 9
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 6
. (RatType)ratType[0] = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . PICHInfo
. . . . PICH_Info
. . . . . fdd
. . . . . . (IntegerType)channelisationCode256[-1] = 2
. . . . . . (PI_CountPerFrame)pi_CountPerFrame[0] = 0
. . . . . . (BooleanType)sttd_Indicator = FALSE
. . . . (IntegerType)dl_TxPower[-1] = -5
. . . . (IntegerType)sccpchId_associated[-1] = 5
- Constraint:
ca_PICH_Info
- BinaryMessage:
30 1e 02 01 00 02 01 06 0a 01 00 30 13 30 11 30 09 02 01 02 0a 01 00 01 01 00 02 01 fb 02 01 05

- No.: 197
- Timestamp: 17:11:01:474_0
- RFN: 2919
- Chip: 27904
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_PCH_FACH_CCCH_Cfg LINE 10
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 6
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 06

- No.: 205
- Timestamp: 17:11:01:476_0
- RFN: 2919
- Chip: 34304
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_RACH_CCCH_Cfg LINE 3
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 7
. (RatType)ratType[0] = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . AICHInfo
. . . . AICH_Info
. . . . . (IntegerType)channelisationCode256[-1] = 3
. . . . . (BooleanType)sttd_Indicator = FALSE
. . . . . (AICH_TransmissionTiming)aich_TransmissionTiming[0] = 0
. . . . (IntegerType)dl_TxPower[-1] = -5
- Constraint:
ca_AichInfo
- BinaryMessage:
30 1b 02 01 00 02 01 07 0a 01 00 30 10 30 0e 30 09 02 01 03 01 01 00 0a 01 00 02 01 fb

- No.: 209
- Timestamp: 17:11:01:482_0
- RFN: 2920
- Chip: 19968
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_RACH_CCCH_Cfg LINE 4
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 7
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 07

- No.: 210
- Timestamp: 17:11:01:483_0
- RFN: 2920
- Chip: 23552
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_RACH_CCCH_Cfg LINE 5
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 8
. (RatType)ratType[0] = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . PRACHInfo
. . . . fdd_tdd
. . . . . fdd
. . . . . . (BitStringType)preambleSignature[16] = "0000000011111111"
. . . . . . (SF_PRACH)spreadingFactorForDataPart[0] = 1
. . . . . . (IntegerType)preambleScramblingCode[-1] = 0
. . . . . . (PuncturingLimit)puncturingLimit[0] = 15
. . . . . . (BitStringType)accessSlot[12] = "111111111111"
- Constraint:
ca_PRACH_Info
- BinaryMessage:
30 22 02 01 00 02 01 08 0a 01 00 30 17 30 15 30 13 03 03 00 00 ff 0a 01 01 02 01 00 0a 01 0f 03 03 04 ff f0

- No.: 214
- Timestamp: 17:11:01:489_0
- RFN: 2921
- Chip: 6656
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_RACH_CCCH_Cfg LINE 6
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 8
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 08

- No.: 215
- Timestamp: 17:11:01:491_0
- RFN: 2921
- Chip: 14592
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Config_REQ
- Source: ts_SS_RACH_CCCH_Cfg LINE 7
- Message Structure:
CPHY_TrCH_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 8
. (RatType)ratType[0] = 0
. TrChConfigType
. CphyTrchConfigReq
. . SS_ActivationTime
. . ulconnectedTrCHList
. . . CphyTrchConfigReq_setseq_0
. . . . (IntegerType)trchid[-1] = 15
. . . . (SS_UL_TransportChannelType)ul_TransportChannelType[0] = 1
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size[-1] = 168
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size[-1] = 360
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional[0] = 0
. . . . . . (IntegerType)rateMatchingAttribute[-1] = 150
. . . . . . (CRC_Size)crc_Size[0] = 3
. . TFCS
. . . ExplicitTFCS_Configuration
. . . . TFCS_ReconfAdd
. . . . . ctfcSize
. . . . . . ctfc2Bit
. . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . (IntegerType)ctfc2[-1] = 0
. . . . . . . . PowerOffsetInformation
. . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . (IntegerType)ctfc2[-1] = 1
. . . . . . . . PowerOffsetInformation
. . dlconnectedTrCHList
. . TFCS
- Constraint:
cab_RACH_InfoActNow
- BinaryMessage:
30 4f 02 01 00 02 01 08 0a 01 00 05 00 30 42 05 00 30 30 30 2e 02 01 0f 0a 01 01 30 26 30 18 30 0a 02 02 00 a8 30 02 05 00 05 00 30 0a 02 02 01 68 30 02 05 00 05 00 30 0a 0a 01 00 02 02 00 96 0a 01 03 30 0c 30 0a 30 03 02 01 00 30 03 02 01 01

- No.: 219
- Timestamp: 17:11:01:502_0
- RFN: 2922
- Chip: 18432
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Config_CNF
- Source: ts_SS_RACH_CCCH_Cfg LINE 8
- Message Structure:
CPHY_TrCH_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 8
- Constraint:
ca_TrChCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 08

- No.: 220
- Timestamp: 17:11:01:505_0
- RFN: 2922
- Chip: 30976
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_SS_RACH_CCCH_Cfg LINE 9
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 8
. (RatType)ratType[0] = 0
. configMessage
. . CmacConfigReq
. . . SS_ActivationTime
. . . UE_Info
. . . . U_RNTI
. . . . (BitStringType)c_RNTI[16] = -
. . . TrCHInfo
. . . . ulconnectedTrCHList
. . . . . TrCHInfo_setseq_0
. . . . . . (IntegerType)trchid[-1] = 15
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size[-1] = 168
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size[-1] = 360
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional[0] = 0
. . . . . . . . (IntegerType)rateMatchingAttribute[-1] = 150
. . . . . . . . (CRC_Size)crc_Size[0] = 3
. . . . TFCS
. . . . . ExplicitTFCS_Configuration
. . . . . . TFCS_ReconfAdd
. . . . . . . ctfcSize
. . . . . . . . ctfc2Bit
. . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . (IntegerType)ctfc2[-1] = 0
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . (IntegerType)ctfc2[-1] = 1
. . . . . . . . . . PowerOffsetInformation
. . . . dlconnectedTrCHList
. . . . TFCS
. . . TrCH_LogCHMappingList1
. . . . ulconnectedTrCHList
. . . . . TrCH_LogCHMappingList1_setseq_0
. . . . . . (IntegerType)trchid[-1] = 15
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation[0] = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType[0] = 1
. . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 5
. . . . . . . . . . (LogicalChannelType)logicalChannelType[0] = 2
. . . . . . . . (IntegerType)rB_Identity[-1] = 0
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
. . . . dlconnectedTrCHList
- Constraint:
ca_CMAC_CfgInfo
- BinaryMessage:
30 6c 02 01 00 02 01 08 0a 01 00 30 61 05 00 30 00 30 3d 30 2d 30 2b 02 01 0f 30 26 30 18 30 0a 02 02 00 a8 30 02 05 00 05 00 30 0a 02 02 01 68 30 02 05 00 05 00 30 0a 0a 01 00 02 02 00 96 0a 01 03 30 0c 30 0a 30 03 02 01 00 30 03 02 01 01 30 1c 30 1a 30 18 02 01 0f 30 13 30 11 30 0c 0a 01 00 0a 01 01 02 01 05 0a 01 02 02 01 00

- No.: 224
- Timestamp: 17:11:01:507_0
- RFN: 2923
- Chip: 1536
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_SS_RACH_CCCH_Cfg LINE 10
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 8
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 08

- No.: 261
- Timestamp: 17:11:01:513_0
- RFN: 2923
- Chip: 25600
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_1DCH_DCCH_Cfg LINE 4
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 26
. (RatType)ratType[0] = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . DPCHInfo
. . . . UL_DPCH_Info
. . . . DL_DPCHInfo
. . . . . DL_CommonInformation
. . . . . . DL_DPCH_InfoCommon
. . . . . . . cfnHandling
. . . . . . . . initialise
. . . . . . . . . (IntegerType)cfntargetsfnframeoffset[-1] = -
. . . . . . . modeSpecificInfo
. . . . . . . . fdd
. . . . . . . . . DL_DPCH_PowerControlInfo
. . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . fdd
. . . . . . . . . . . . (DPC_Mode)dpc_Mode[0] = 0
. . . . . . . . . (IntegerType)powerOffsetPilot_pdpdch[-1] = 0
. . . . . . . . . Dl_rate_matching_restriction
. . . . . . . . . SF512_AndPilot
. . . . . . . . . . (PilotBits128)sfd128[0] = 0
. . . . . . . . . (PositionFixedOrFlexible)positionFixedOrFlexible[0] = 0
. . . . . . . . . (BooleanType)tfci_Existence = FALSE
. . . . . . modeSpecificInfo
. . . . . . . fdd
. . . . . . . . (IntegerType)defaultDPCH_OffsetValue[-1] = 459
. . . . . . . . DPCH_CompressedModeInfo
. . . . . . . . (TX_DiversityMode)tx_DiversityMode[0] = 0
. . . . . . . . SSDT_Information
. . . . . DL_DPCH_InfoPerRL
. . . . . . fdd
. . . . . . . (PCPICH_UsageForChannelEst)pCPICH_UsageForChannelEst[0] = 0
. . . . . . . (IntegerType)dpch_FrameOffset[-1] = 18
. . . . . . . SecondaryCPICH_Info
. . . . . . . DL_ChannelisationCodeList
. . . . . . . . DL_ChannelisationCode
. . . . . . . . . (IntegerType)secondaryScramblingCode[-1] = 1
. . . . . . . . . SF512_AndCodeNumber
. . . . . . . . . . (IntegerType)sf128[-1] = 0
. . . . . . . . . (ScramblingCodeChange)scramblingCodeChange[0] = -
. . . . . . . (IntegerType)tpc_CombinationIndex[-1] = 0
. . . . . . . (SSDT_CellIdentity)ssdt_CellIdentity[0] = -
. . . . . . . (ClosedLoopTimingAdjMode)closedLoopTimingAdjMode[0] = -
. . . . . (IntegerType)powerOffsetOfTFCI_PO1[-1] = 0
. . . . . (IntegerType)powerOffsetOfTPC_PO2[-1] = 0
. . . . . (IntegerType)powerOffsetOfPILOT_PO3[-1] = 0
. . . . . (IntegerType)dl_TxPower[-1] = -5
. . . . . (IntegerType)dl_TxPowerMax[-1] = 15
. . . . . (IntegerType)dl_TxPowerMin[-1] = -35
- Constraint:
ca_DL_DPCH_Info
- BinaryMessage:
30 5a 02 01 00 02 01 1a 0a 01 00 30 4f 30 4d 30 4b 30 22 30 17 30 00 30 13 30 05 30 03 0a 01 00 02 01 00 0a 01 00 0a 01 00 01 01 00 30 07 02 02 01 cb 0a 01 00 30 13 0a 01 00 02 01 12 30 08 30 06 02 01 01 02 01 00 02 01 00 02 01 00 02 01 00 02 01 00 02 01 fb 02 01 0f 02 01 dd

- No.: 265
- Timestamp: 17:11:01:523_0
- RFN: 2924
- Chip: 23040
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_1DCH_DCCH_Cfg LINE 5
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 26
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 1a

- No.: 266
- Timestamp: 17:11:01:525_0
- RFN: 2924
- Chip: 33024
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Config_REQ
- Source: ts_SS_1DCH_DCCH_Cfg LINE 6
- Message Structure:
CPHY_TrCH_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 26
. (RatType)ratType[0] = 0
. TrChConfigType
. . (TrChConfigType_list_0)dch[0] = 0
. CphyTrchConfigReq
. . SS_ActivationTime
. . ulconnectedTrCHList
. . TFCS
. . dlconnectedTrCHList
. . . CphyTrchConfigReq_setseq_1
. . . . (IntegerType)trchid[-1] = 10
. . . . (SS_DL_TransportChannelType)dl_TransportChannelType[0] = 0
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size[-1] = 148
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional[0] = 1
. . . . . . (IntegerType)rateMatchingAttribute[-1] = 192
. . . . . . (CRC_Size)crc_Size[0] = 3
. . TFCS
. . . ExplicitTFCS_Configuration
. . . . TFCS_ReconfAdd
. . . . . ctfcSize
. . . . . . ctfc2Bit
. . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . (IntegerType)ctfc2[-1] = 0
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . (IntegerType)ctfc2[-1] = 1
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . fdd
. . . . . . . . . . . . . (IntegerType)gainFactorBetaC[-1] = 11
. . . . . . . . . . . (IntegerType)gainFactorBetaD[-1] = 15
. . . . . . . . . . . (IntegerType)referenceTFC_ID[-1] = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
- Constraint:
ca_DCH_148_TTI_10_DL_InfoActNow
- BinaryMessage:
30 5a 02 01 00 02 01 1a 0a 01 00 0a 01 00 30 4c 05 00 30 26 30 24 02 01 0a 0a 01 00 30 1c 30 0e 30 0c 02 02 00 94 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 c0 0a 01 03 30 20 30 1e 30 08 02 01 00 30 03 02 01 00 30 12 02 01 01 30 0d 30 0b 30 03 02 01 0b 02 01 0f 02 01 00

- No.: 270
- Timestamp: 17:11:01:534_0
- RFN: 2925
- Chip: 29440
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Config_CNF
- Source: ts_SS_1DCH_DCCH_Cfg LINE 7
- Message Structure:
CPHY_TrCH_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 26
- Constraint:
ca_TrChCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 1a

- No.: 271
- Timestamp: 17:11:01:541_0
- RFN: 2926
- Chip: 15872
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_SS_1DCH_DCCH_Cfg LINE 8
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 26
. (RatType)ratType[0] = 0
. configMessage
. . CmacConfigReq
. . . SS_ActivationTime
. . . UE_Info
. . . . U_RNTI
. . . . (BitStringType)c_RNTI[16] = -
. . . TrCHInfo
. . . . ulconnectedTrCHList
. . . . TFCS
. . . . dlconnectedTrCHList
. . . . . TrCHInfo_setseq_1
. . . . . . (IntegerType)trchid[-1] = 10
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size[-1] = 148
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional[0] = 1
. . . . . . . . (IntegerType)rateMatchingAttribute[-1] = 192
. . . . . . . . (CRC_Size)crc_Size[0] = 3
. . . . TFCS
. . . . . ExplicitTFCS_Configuration
. . . . . . TFCS_ReconfAdd
. . . . . . . ctfcSize
. . . . . . . . ctfc2Bit
. . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . (IntegerType)ctfc2[-1] = 0
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . (IntegerType)ctfc2[-1] = 1
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC[-1] = 11
. . . . . . . . . . . . . (IntegerType)gainFactorBetaD[-1] = 15
. . . . . . . . . . . . . (IntegerType)referenceTFC_ID[-1] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . TrCH_LogCHMappingList1
. . . . ulconnectedTrCHList
. . . . dlconnectedTrCHList
. . . . . TrCH_LogCHMappingList1_setseq_1
. . . . . . (IntegerType)trchid[-1] = 10
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation[0] = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType[0] = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . . . (LogicalChannelType)logicalChannelType[0] = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 1
. . . . . . . . (IntegerType)rB_Identity[-1] = 1
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation[0] = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType[0] = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 2
. . . . . . . . . . (LogicalChannelType)logicalChannelType[0] = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 2
. . . . . . . . (IntegerType)rB_Identity[-1] = 2
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation[0] = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType[0] = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 3
. . . . . . . . . . (LogicalChannelType)logicalChannelType[0] = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 3
. . . . . . . . (IntegerType)rB_Identity[-1] = 3
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation[0] = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType[0] = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 4
. . . . . . . . . . (LogicalChannelType)logicalChannelType[0] = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 4
. . . . . . . . (IntegerType)rB_Identity[-1] = 4
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_CMAC_CfgInfo
- BinaryMessage:
30 81 c4 02 01 ff 02 01 1a 0a 01 00 30 81 b8 05 00 30 00 30 47 30 23 30 21 02 01 0a 30 1c 30 0e 30 0c 02 02 00 94 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 c0 0a 01 03 30 20 30 1e 30 08 02 01 00 30 03 02 01 00 30 12 02 01 01 30 0d 30 0b 30 03 02 01 0b 02 01 0f 02 01 00 30 69 30 67 30 65 02 01 0a 30 60 30 16 30 11 0a 01 00 0a 01 00 02 01 01 0a 01 04 05 00 02 01 01 02 01 01 30 16 30 11 0a 01 00 0a 01 00 02 01 02 0a 01 04 05 00 02 01 02 02 01 02 30 16 30 11 0a 01 00 0a 01 00 02 01 03 0a 01 04 05 00 02 01 03 02 01 03 30 16 30 11 0a 01 00 0a 01 00 02 01 04 0a 01 04 05 00 02 01 04 02 01 04

- No.: 275
- Timestamp: 17:11:01:553_0
- RFN: 2927
- Chip: 24320
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_SS_1DCH_DCCH_Cfg LINE 9
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 26
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 1a

- No.: 276
- Timestamp: 17:11:01:554_0
- RFN: 2927
- Chip: 29184
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_1DCH_DCCH_Cfg LINE 10
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 20
. (RatType)ratType[0] = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . DPCHInfo
. . . . UL_DPCH_Info
. . . . . UL_DPCH_PowerControlInfo
. . . . . . fdd
. . . . . . . (IntegerType)dpcch_PowerOffset[-1] = -40
. . . . . . . (IntegerType)pc_Preamble[-1] = 1
. . . . . . . (IntegerType)sRB_delay[-1] = 7
. . . . . . . PowerControlAlgorithm
. . . . . . . . (IntegerType)algorithm1[-1] = 1
. . . . . modeSpecificInfo
. . . . . . fdd
. . . . . . . (ScramblingCodeType)scramblingCodeType[0] = 1
. . . . . . . (IntegerType)scramblingCode[-1] = 0
. . . . . . . (IntegerType)numberOfDPDCH[-1] = -
. . . . . . . (SpreadingFactor)spreadingFactor[0] = 4
. . . . . . . (BooleanType)tfci_Existence = TRUE
. . . . . . . (IntegerType)numberOfFBI_Bits[-1] = -
. . . . . . . (PuncturingLimit)puncturingLimit[0] = 15
. . . . DL_DPCHInfo
- Constraint:
ca_UL_DPCH_Info
- BinaryMessage:
30 2e 02 01 00 02 01 14 0a 01 00 30 23 30 21 30 1f 30 0c 02 01 d8 02 01 01 02 01 07 02 01 01 30 0f 0a 01 01 02 01 00 0a 01 04 01 01 ff 0a 01 0f

- No.: 280
- Timestamp: 17:11:01:564_0
- RFN: 2928
- Chip: 27648
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_1DCH_DCCH_Cfg LINE 11
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 20
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 281
- Timestamp: 17:11:01:566_0
- RFN: 2928
- Chip: 35328
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Config_REQ
- Source: ts_SS_1DCH_DCCH_Cfg LINE 12
- Message Structure:
CPHY_TrCH_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 20
. (RatType)ratType[0] = 0
. TrChConfigType
. . (TrChConfigType_list_0)dch[0] = 0
. CphyTrchConfigReq
. . SS_ActivationTime
. . ulconnectedTrCHList
. . . CphyTrchConfigReq_setseq_0
. . . . (IntegerType)trchid[-1] = 5
. . . . (SS_UL_TransportChannelType)ul_TransportChannelType[0] = 0
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size[-1] = 148
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional[0] = 1
. . . . . . (IntegerType)rateMatchingAttribute[-1] = 192
. . . . . . (CRC_Size)crc_Size[0] = 3
. . TFCS
. . . ExplicitTFCS_Configuration
. . . . TFCS_ReconfAdd
. . . . . ctfcSize
. . . . . . ctfc2Bit
. . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . (IntegerType)ctfc2[-1] = 0
. . . . . . . . PowerOffsetInformation
. . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . (IntegerType)ctfc2[-1] = 1
. . . . . . . . PowerOffsetInformation
. . dlconnectedTrCHList
. . TFCS
- Constraint:
ca_DCH_148_TTI_10_UL_InfoActNow
- BinaryMessage:
30 46 02 01 00 02 01 14 0a 01 00 0a 01 00 30 38 05 00 30 26 30 24 02 01 05 0a 01 00 30 1c 30 0e 30 0c 02 02 00 94 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 c0 0a 01 03 30 0c 30 0a 30 03 02 01 00 30 03 02 01 01

- No.: 285
- Timestamp: 17:11:01:574_0
- RFN: 2929
- Chip: 29184
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Config_CNF
- Source: ts_SS_1DCH_DCCH_Cfg LINE 13
- Message Structure:
CPHY_TrCH_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 20
- Constraint:
ca_TrChCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 286
- Timestamp: 17:11:01:578_0
- RFN: 2930
- Chip: 5632
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_SS_1DCH_DCCH_Cfg LINE 14
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 20
. (RatType)ratType[0] = 0
. configMessage
. . CmacConfigReq
. . . SS_ActivationTime
. . . UE_Info
. . . . U_RNTI
. . . . (BitStringType)c_RNTI[16] = -
. . . TrCHInfo
. . . . ulconnectedTrCHList
. . . . . TrCHInfo_setseq_0
. . . . . . (IntegerType)trchid[-1] = 5
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size[-1] = 148
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional[0] = 1
. . . . . . . . (IntegerType)rateMatchingAttribute[-1] = 192
. . . . . . . . (CRC_Size)crc_Size[0] = 3
. . . . TFCS
. . . . . ExplicitTFCS_Configuration
. . . . . . TFCS_ReconfAdd
. . . . . . . ctfcSize
. . . . . . . . ctfc2Bit
. . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . (IntegerType)ctfc2[-1] = 0
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . (IntegerType)ctfc2[-1] = 1
. . . . . . . . . . PowerOffsetInformation
. . . . dlconnectedTrCHList
. . . . TFCS
. . . TrCH_LogCHMappingList1
. . . . ulconnectedTrCHList
. . . . . TrCH_LogCHMappingList1_setseq_0
. . . . . . (IntegerType)trchid[-1] = 5
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation[0] = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType[0] = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . . . (LogicalChannelType)logicalChannelType[0] = 4
. . . . . . . . (IntegerType)rB_Identity[-1] = 1
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation[0] = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType[0] = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 2
. . . . . . . . . . (LogicalChannelType)logicalChannelType[0] = 4
. . . . . . . . (IntegerType)rB_Identity[-1] = 2
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation[0] = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType[0] = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 3
. . . . . . . . . . (LogicalChannelType)logicalChannelType[0] = 4
. . . . . . . . (IntegerType)rB_Identity[-1] = 3
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation[0] = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType[0] = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 4
. . . . . . . . . . (LogicalChannelType)logicalChannelType[0] = 4
. . . . . . . . (IntegerType)rB_Identity[-1] = 4
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
. . . . dlconnectedTrCHList
- Constraint:
ca_CMAC_CfgInfo
- BinaryMessage:
30 81 9c 02 01 ff 02 01 14 0a 01 00 30 81 90 05 00 30 00 30 33 30 23 30 21 02 01 05 30 1c 30 0e 30 0c 02 02 00 94 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 c0 0a 01 03 30 0c 30 0a 30 03 02 01 00 30 03 02 01 01 30 55 30 53 30 51 02 01 05 30 4c 30 11 30 0c 0a 01 00 0a 01 00 02 01 01 0a 01 04 02 01 01 30 11 30 0c 0a 01 00 0a 01 00 02 01 02 0a 01 04 02 01 02 30 11 30 0c 0a 01 00 0a 01 00 02 01 03 0a 01 04 02 01 03 30 11 30 0c 0a 01 00 0a 01 00 02 01 04 0a 01 04 02 01 04

- No.: 290
- Timestamp: 17:11:01:590_0
- RFN: 2931
- Chip: 14336
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_SS_1DCH_DCCH_Cfg LINE 15
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 20
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 14

- No.: 293
- Timestamp: 17:11:01:591_1
- RFN: 2931
- Chip: 19456
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB_BCCH_BCH_Cfg LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 246
. . . . . UL_RLC_Mode
. . . . . . UL_TM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . (BooleanType)segmentationIndication = FALSE
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[0] = -
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 1
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_BCCH_Info
- BinaryMessage:
30 1d 02 01 00 02 01 ff 0a 01 00 30 12 30 0b 30 09 02 02 00 f6 30 03 01 01 00 30 03 02 01 01

- No.: 297
- Timestamp: 17:11:01:595_0
- RFN: 2931
- Chip: 30976
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB_BCCH_BCH_Cfg LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 300
- Timestamp: 17:11:01:596_0
- RFN: 2931
- Chip: 35840
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB_PCCH_Cfg LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -2
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 240
. . . . . UL_RLC_Mode
. . . . . . UL_TM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . (BooleanType)segmentationIndication = FALSE
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[0] = -
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 1
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_PCCH_Info
- BinaryMessage:
30 1d 02 01 00 02 01 fe 0a 01 00 30 12 30 0b 30 09 02 02 00 f0 30 03 01 01 00 30 03 02 01 01

- No.: 304
- Timestamp: 17:11:01:600_0
- RFN: 2932
- Chip: 14848
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB_PCCH_Cfg LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 fe

- No.: 307
- Timestamp: 17:11:01:602_0
- RFN: 2932
- Chip: 19968
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB0_Cfg LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 0
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 152
. . . . . UL_RLC_Mode
. . . . . . UL_UM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (NoExplicitDiscard)timerBasedNoExplicit[0] = 9
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[0] = -
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 5
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_UM_DL_Info
- BinaryMessage:
30 1d 02 01 00 02 01 00 0a 01 00 30 12 30 0b 30 09 02 02 00 98 30 03 0a 01 09 30 03 02 01 05

- No.: 311
- Timestamp: 17:11:01:605_0
- RFN: 2932
- Chip: 31488
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB0_Cfg LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 0
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 00

- No.: 312
- Timestamp: 17:11:01:606_0
- RFN: 2932
- Chip: 36096
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB0_Cfg LINE 3
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 0
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_TM_RLC_Mode
. . . . . . (BooleanType)segmentationIndication = FALSE
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 166
. . . . . UL_RLC_Mode
. . . . . . UL_TM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . (BooleanType)segmentationIndication = FALSE
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 5
. . . . (IntegerType)dLlogicalChannelIdentity[0] = -
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_TM_UL_Info
- BinaryMessage:
30 22 02 01 00 02 01 00 0a 01 00 30 17 30 10 30 03 01 01 00 30 09 02 02 00 a6 30 03 01 01 00 30 03 02 01 05

- No.: 316
- Timestamp: 17:11:01:612_0
- RFN: 2933
- Chip: 23040
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB0_Cfg LINE 4
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 0
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 00

- No.: 319
- Timestamp: 17:11:01:614_0
- RFN: 2933
- Chip: 28672
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 1
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 136
. . . . . UL_RLC_Mode
. . . . . . UL_UM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (NoExplicitDiscard)timerBasedNoExplicit[0] = 9
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 1
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 1
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_UM_Info
- BinaryMessage:
30 22 02 01 ff 02 01 01 0a 01 00 30 17 30 0d 05 00 30 09 02 02 00 88 30 03 0a 01 09 30 06 02 01 01 02 01 01

- No.: 323
- Timestamp: 17:11:01:620_0
- RFN: 2934
- Chip: 14592
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 324
- Timestamp: 17:11:01:622_0
- RFN: 2934
- Chip: 21248
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 3
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 2
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 2
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 2
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 02 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 13 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 02 02 01 02

- No.: 328
- Timestamp: 17:11:01:634_0
- RFN: 2935
- Chip: 28672
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 4
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 329
- Timestamp: 17:11:01:635_0
- RFN: 2935
- Chip: 34816
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 5
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 3
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 3
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 3
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 03 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 13 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 03 02 01 03

- No.: 333
- Timestamp: 17:11:01:650_0
- RFN: 2937
- Chip: 15872
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 6
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 3
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 334
- Timestamp: 17:11:01:652_0
- RFN: 2937
- Chip: 21504
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 7
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 4
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 4
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 4
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 04 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 13 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 04 02 01 04

- No.: 338
- Timestamp: 17:11:01:665_0
- RFN: 2938
- Chip: 35328
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 8
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 4
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 384
- Timestamp: 17:11:01:677_0
- RFN: 2940
- Chip: 256
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 27
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 1b

- No.: 389
- Timestamp: 17:11:01:682_0
- RFN: 2940
- Chip: 19712
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendNoSegDefSchedul LINE 2
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 390
- Timestamp: 17:11:01:683_0
- RFN: 2940
- Chip: 22272
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendNoSegDefSchedul LINE 3
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 08 02 01 00 02 01 ff 00 00

- No.: 398
- Timestamp: 17:11:01:686_0
- RFN: 2940
- Chip: 34560
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 11
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 0b

- No.: 403
- Timestamp: 17:11:01:693_0
- RFN: 2941
- Chip: 20992
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB1 LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 404
- Timestamp: 17:11:01:693_1
- RFN: 2941
- Chip: 24320
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB1 LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 1
. . . . . . . (BitStringType)sib_Data_variable[-1] = "1100010000000000000001011000100000101000000000100001000000010000000101000000000000000000000011000111010000"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 2
. . . . . . . (BitStringType)sib_Data_variable[-1] = "00000000000000000001"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 1c 02 01 00 02 01 ff 00 0e 21 69 c4 00 05 88 28 02 10 10 14 00 00 0c 74 04 26 00 00 20

- No.: 416
- Timestamp: 17:11:01:697_0
- RFN: 2941
- Chip: 37120
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 11
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 0b

- No.: 421
- Timestamp: 17:11:01:712_0
- RFN: 2943
- Chip: 19968
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB2 LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 422
- Timestamp: 17:11:01:713_0
- RFN: 2943
- Chip: 23040
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB2 LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 1
. . . . . . . (BitStringType)sib_Data_variable[-1] = "1100010000000000000001011000100000101000000000100001000000010000000101000000000000000000000011000111010000"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 2
. . . . . . . (BitStringType)sib_Data_variable[-1] = "00000000000000000001"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 1c 02 01 00 02 01 ff 00 0e 21 69 c4 00 05 88 28 02 10 10 14 00 00 0c 74 04 26 00 00 20

- No.: 434
- Timestamp: 17:11:01:716_3
- RFN: 2943
- Chip: 35840
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 10
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 0a

- No.: 439
- Timestamp: 17:11:01:732_0
- RFN: 2945
- Chip: 19712
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB3 LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 440
- Timestamp: 17:11:01:733_0
- RFN: 2945
- Chip: 23552
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB3 LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 7
. . . . . . . (BitStringType)sib_Data_variable[-1] = "100000101000000010000001"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 3
. . . . . . . (BitStringType)sib_Data_variable[-1] = "010000000000000000000000000000001011001100011000000000100100001000000100011111111111111111111111"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 1b 02 01 00 02 01 ff 00 0e 27 17 82 80 81 1a fa 00 00 00 05 98 c0 12 10 23 ff ff f8

- No.: 452
- Timestamp: 17:11:01:736_3
- RFN: 2945
- Chip: 36352
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 26
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 1a

- No.: 457
- Timestamp: 17:11:01:742_0
- RFN: 2946
- Chip: 19968
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB4 LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 458
- Timestamp: 17:11:01:743_0
- RFN: 2946
- Chip: 23296
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB4 LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 7
. . . . . . . (BitStringType)sib_Data_variable[-1] = "100000101000000010000001"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 4
. . . . . . . (BitStringType)sib_Data_variable[-1] = "0000000000000000000000000000000101100110001100000000010010000100000010001110111"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 19 02 01 00 02 01 ff 00 0e 27 17 82 80 81 22 70 00 00 00 0b 31 80 24 20 47 70

- No.: 475
- Timestamp: 17:11:01:751_0
- RFN: 2947
- Chip: 16384
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 23
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 17

- No.: 480
- Timestamp: 17:11:01:753_0
- RFN: 2947
- Chip: 24320
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB5 LINE 41
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 481
- Timestamp: 17:11:01:754_0
- RFN: 2947
- Chip: 26624
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB5 LINE 42
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 08 02 01 00 02 01 ff 00 00

- No.: 485
- Timestamp: 17:11:01:755_0
- RFN: 2947
- Chip: 30464
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 19
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 13

- No.: 490
- Timestamp: 17:11:01:762_0
- RFN: 2948
- Chip: 18944
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB5 LINE 44
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 491
- Timestamp: 17:11:01:763_0
- RFN: 2948
- Chip: 22016
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB5 LINE 45
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . FirstSegment
. . . . . . (SIB_Type)sib_Type[0] = 5
. . . . . . (IntegerType)seg_Count[-1] = 3
. . . . . . (BitStringType)sib_Data_fixed[222] = "000101010100010000111110000000001111111101000011111111111111110111010010000100001111000000101001000011000000101010100101010110000000000000001100110001011011010101111110001010111010000011111110100000111111101000001111111010"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 25 02 01 00 02 01 ff 00 02 52 15 44 3e 00 ff 43 ff fd d2 10 f0 29 0c 0a a5 58 00 0c c5 b5 7e 2b a0 fe 83 fa 0f e8

- No.: 495
- Timestamp: 17:11:01:764_0
- RFN: 2948
- Chip: 26368
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 21
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 15

- No.: 500
- Timestamp: 17:11:01:772_0
- RFN: 2949
- Chip: 19456
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB5 LINE 47
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 501
- Timestamp: 17:11:01:773_0
- RFN: 2949
- Chip: 22272
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB5 LINE 48
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . SubsequentSegment
. . . . . . (SIB_Type)sib_Type[0] = 5
. . . . . . (IntegerType)segmentIndex[-1] = 1
. . . . . . (BitStringType)sib_Data_fixed[222] = "000011111111010000000000000000001101011000110100010000111111010011100101000001100001000011001010000000110000001110001001000000010110000000000000100000001110000000001000100001100100001010011001000010100000000000110000000100"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 25 02 01 00 02 01 ff 00 04 50 0f f4 00 00 d6 34 43 f4 e5 06 10 ca 03 03 89 01 60 00 80 e0 08 86 42 99 0a 00 30 10

- No.: 505
- Timestamp: 17:11:01:774_0
- RFN: 2949
- Chip: 26368
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 22
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 16

- No.: 510
- Timestamp: 17:11:01:782_0
- RFN: 2950
- Chip: 18432
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB5 LINE 50
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 512
- Timestamp: 17:11:01:782_2
- RFN: 2950
- Chip: 21504
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB5 LINE 52
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . LastSegmentShort
. . . . . . (SIB_Type)sib_Type[0] = 5
. . . . . . (IntegerType)segmentIndex[-1] = 2
. . . . . . (BitStringType)sib_Data_variable[-1] = "010001011100101011010110100000000000011110001000011000000001011011011011011000100000000001000011000010001001010000001011011010000000010000"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 1c 02 01 00 02 01 ff 00 06 51 89 45 ca d6 80 07 88 60 16 db 62 00 43 08 94 0b 68 04 00

- No.: 529
- Timestamp: 17:11:01:786_0
- RFN: 2950
- Chip: 35840
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 3
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 03

- No.: 534
- Timestamp: 17:11:01:793_0
- RFN: 2951
- Chip: 22528
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB6 LINE 8
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 537
- Timestamp: 17:11:01:794_0
- RFN: 2951
- Chip: 26368
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB6:lt_CompleteSIB LINE 4
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 6
. . . . . . . (BitStringType)sib_Data_variable[-1] = "0000001010010001"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 0c 02 01 00 02 01 ff 00 0e 06 0f 02 91

- No.: 542
- Timestamp: 17:11:01:795_0
- RFN: 2951
- Chip: 30464
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 5
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 05

- No.: 547
- Timestamp: 17:11:01:801_0
- RFN: 2952
- Chip: 18176
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB6 LINE 11
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 548
- Timestamp: 17:11:01:802_0
- RFN: 2952
- Chip: 20224
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB6 LINE 12
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 08 02 01 00 02 01 ff 00 00

- No.: 552
- Timestamp: 17:11:01:803_1
- RFN: 2952
- Chip: 23808
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 6
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 06

- No.: 557
- Timestamp: 17:11:01:812_0
- RFN: 2953
- Chip: 19456
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB6 LINE 14
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 558
- Timestamp: 17:11:01:812_1
- RFN: 2953
- Chip: 22016
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB6 LINE 15
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 08 02 01 00 02 01 ff 00 00

- No.: 562
- Timestamp: 17:11:01:813_3
- RFN: 2953
- Chip: 25856
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 7
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 07

- No.: 567
- Timestamp: 17:11:01:822_0
- RFN: 2954
- Chip: 19200
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB6 LINE 17
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 568
- Timestamp: 17:11:01:822_1
- RFN: 2954
- Chip: 21248
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB6 LINE 18
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 08 02 01 00 02 01 ff 00 00

- No.: 576
- Timestamp: 17:11:01:825_0
- RFN: 2954
- Chip: 31232
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 2
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 02

- No.: 581
- Timestamp: 17:11:01:832_0
- RFN: 2955
- Chip: 20992
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB7 LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 584
- Timestamp: 17:11:01:833_1
- RFN: 2955
- Chip: 26112
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB7:lt_CompleteSIB LINE 4
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 7
. . . . . . . (BitStringType)sib_Data_variable[-1] = "100000101000000010000001"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 0d 02 01 00 02 01 ff 00 0e 07 17 82 80 81

- No.: 592
- Timestamp: 17:11:01:837_0
- RFN: 2956
- Chip: 0
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 10
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 0a

- No.: 597
- Timestamp: 17:11:01:852_0
- RFN: 2957
- Chip: 20736
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB7:lt_ConcatWithSIB3 LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 598
- Timestamp: 17:11:01:853_0
- RFN: 2957
- Chip: 24832
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB7:lt_ConcatWithSIB3 LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 7
. . . . . . . (BitStringType)sib_Data_variable[-1] = "100000101000000010000001"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 3
. . . . . . . (BitStringType)sib_Data_variable[-1] = "010000000000000000000000000000001011001100011000000000100100001000000100011111111111111111111111"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 1b 02 01 00 02 01 ff 00 0e 27 17 82 80 81 1a fa 00 00 00 05 98 c0 12 10 23 ff ff f8

- No.: 606
- Timestamp: 17:11:01:856_0
- RFN: 2957
- Chip: 36096
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 18
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 12

- No.: 611
- Timestamp: 17:11:01:862_0
- RFN: 2958
- Chip: 19456
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB7:lt_ConcatWithSIB18 LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 612
- Timestamp: 17:11:01:863_0
- RFN: 2958
- Chip: 23296
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB7:lt_ConcatWithSIB18 LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 7
. . . . . . . (BitStringType)sib_Data_variable[-1] = "100000101000000010000001"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 26
. . . . . . . (BitStringType)sib_Data_variable[-1] = "100000"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 10 02 01 00 02 01 ff 00 0e 27 17 82 80 81 d0 2c 00

- No.: 620
- Timestamp: 17:11:01:865_3
- RFN: 2958
- Chip: 34048
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 26
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 1a

- No.: 625
- Timestamp: 17:11:01:873_0
- RFN: 2959
- Chip: 23296
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB7:lt_ConcatWithSIB4 LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 626
- Timestamp: 17:11:01:873_1
- RFN: 2959
- Chip: 26880
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB7:lt_ConcatWithSIB4 LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 7
. . . . . . . (BitStringType)sib_Data_variable[-1] = "100000101000000010000001"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 4
. . . . . . . (BitStringType)sib_Data_variable[-1] = "0000000000000000000000000000000101100110001100000000010010000100000010001110111"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 19 02 01 00 02 01 ff 00 0e 27 17 82 80 81 22 70 00 00 00 0b 31 80 24 20 47 70

- No.: 640
- Timestamp: 17:11:01:878_0
- RFN: 2960
- Chip: 4096
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 31
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 1f

- No.: 645
- Timestamp: 17:11:01:883_0
- RFN: 2960
- Chip: 23552
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB11 LINE 20
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 646
- Timestamp: 17:11:01:883_1
- RFN: 2960
- Chip: 25856
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB11 LINE 21
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 08 02 01 00 02 01 ff 00 00

- No.: 650
- Timestamp: 17:11:01:884_2
- RFN: 2960
- Chip: 29440
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 29
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 1d

- No.: 655
- Timestamp: 17:11:01:892_0
- RFN: 2961
- Chip: 19712
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB11 LINE 23
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 656
- Timestamp: 17:11:01:892_1
- RFN: 2961
- Chip: 23040
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB11 LINE 24
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . FirstSegment
. . . . . . (SIB_Type)sib_Type[0] = 11
. . . . . . (IntegerType)seg_Count[-1] = 2
. . . . . . (BitStringType)sib_Data_fixed[222] = "001000001101100100010010000000001000110010000100001000010010010110101000100000100110010001010011000001011001000010100111000010111000010100001000100010001100100101010100000001001010000101001010100001100001001010001000001010"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 25 02 01 00 02 01 ff 00 02 b1 20 d9 12 00 8c 84 21 25 a8 82 64 53 05 90 a7 0b 85 08 88 c9 54 04 a1 4a 86 12 88 28

- No.: 660
- Timestamp: 17:11:01:894_0
- RFN: 2961
- Chip: 27392
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 30
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 1e

- No.: 665
- Timestamp: 17:11:01:901_0
- RFN: 2962
- Chip: 18688
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB11 LINE 26
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 667
- Timestamp: 17:11:01:902_1
- RFN: 2962
- Chip: 22016
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB11 LINE 28
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . LastSegmentShort
. . . . . . (SIB_Type)sib_Type[0] = 11
. . . . . . (IntegerType)segmentIndex[-1] = 1
. . . . . . (BitStringType)sib_Data_variable[-1] = "00010000110000100101001001101010100001100001001010100010110001101100101010000011001101101000100001001111101000100010000001010010110000100010100001010101111000"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 1e 02 01 00 02 01 ff 00 06 b0 9d 10 c2 52 6a 86 12 a2 c6 ca 83 36 88 4f a2 20 52 c2 28 55 e0

- No.: 680
- Timestamp: 17:11:01:905_2
- RFN: 2962
- Chip: 34816
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 13
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 0d

- No.: 685
- Timestamp: 17:11:01:912_0
- RFN: 2963
- Chip: 19712
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB12 LINE 8
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 688
- Timestamp: 17:11:01:913_0
- RFN: 2963
- Chip: 23552
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB12:lt_CompleteSIB LINE 4
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 12
. . . . . . . (BitStringType)sib_Data_variable[-1] = "000000000"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 0c 02 01 00 02 01 ff 00 0e 0c 08 00 00

- No.: 693
- Timestamp: 17:11:01:914_0
- RFN: 2963
- Chip: 27648
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 14
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 0e

- No.: 698
- Timestamp: 17:11:01:921_0
- RFN: 2964
- Chip: 18688
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB12 LINE 11
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 699
- Timestamp: 17:11:01:922_0
- RFN: 2964
- Chip: 20992
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB12 LINE 12
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 08 02 01 00 02 01 ff 00 00

- No.: 703
- Timestamp: 17:11:01:923_0
- RFN: 2964
- Chip: 24576
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 15
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 0f

- No.: 708
- Timestamp: 17:11:01:932_0
- RFN: 2965
- Chip: 20480
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB12 LINE 14
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 709
- Timestamp: 17:11:01:932_1
- RFN: 2965
- Chip: 23040
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB12 LINE 15
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 08 02 01 00 02 01 ff 00 00

- No.: 717
- Timestamp: 17:11:01:935_0
- RFN: 2965
- Chip: 33536
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 18
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 12

- No.: 722
- Timestamp: 17:11:01:941_0
- RFN: 2966
- Chip: 18944
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB18 LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 723
- Timestamp: 17:11:01:942_0
- RFN: 2966
- Chip: 21760
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB18 LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 7
. . . . . . . (BitStringType)sib_Data_variable[-1] = "100000101000000010000001"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 26
. . . . . . . (BitStringType)sib_Data_variable[-1] = "100000"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 10 02 01 00 02 01 ff 00 0e 27 17 82 80 81 d0 2c 00

- No.: 735
- Timestamp: 17:11:01:945_0
- RFN: 2966
- Chip: 33280
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 4
. . (IntegerType)sg_POS[-1] = 1
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 04 02 01 01

- No.: 740
- Timestamp: 17:11:01:951_0
- RFN: 2967
- Chip: 19968
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSB1_DefSchedul LINE 4
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 743
- Timestamp: 17:11:01:953_0
- RFN: 2967
- Chip: 24064
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSB1_DefSchedul:lt_CompleteSIB LINE 4
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 27
. . . . . . . (BitStringType)sib_Data_variable[-1] = "00010000101010001000001100110000010010010100111000101001110100000000010110100010001101110010100010010010"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 17 02 01 00 02 01 ff 00 0e 1b 67 10 a8 83 30 49 4e 29 d0 05 a2 37 28 92

- No.: 761
- Timestamp: 17:11:01:956_4
- RFN: 2968
- Chip: 768
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 3
. . (IntegerType)sg_POS[-1] = 0
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 03 02 01 00

- No.: 766
- Timestamp: 17:11:01:962_0
- RFN: 2968
- Chip: 23040
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendMIB LINE 7
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 769
- Timestamp: 17:11:01:963_1
- RFN: 2968
- Chip: 27136
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendMIB:lt_CompleteSIB LINE 4
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 0
. . . . . . . (BitStringType)sib_Data_variable[-1] = "0000000000000000010000000010010110101010000100010000000000001000100010110000101000100010110001001000100010100001101000100110100010001110010010010011000100010000"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 1e 02 01 00 02 01 ff 00 0e 00 9f 00 00 40 25 aa 11 00 08 8b 0a 22 c4 88 a1 a2 68 8e 49 31 10

- No.: 786
- Timestamp: 17:11:01:966_0
- RFN: 2968
- Chip: 36608
- Event: Send
- PCO: Ut
- Message: MMI_CmdReq
- Source: ts_MMI_UE_SwitchOn LINE 2
- Message Structure:
MMI_CmdReq
. (IA5StringType)cmd[-1] = "Please switch on the UE"
- Constraint:
ca_MMI_CmdReq
- BinaryMessage:
50 6c 65 61 73 65 20 73 77 69 74 63 68 20 6f 6e 20 74 68 65 20 55 45

- No.: 790
- Timestamp: 17:11:05:844_0
- RFN: 3356
- Chip: 27392
- Event: Receive
- PCO: Ut
- Message: MMI_CmdCnf
- Source: ts_MMI_UE_SwitchOn LINE 3
- Message Structure:
MMI_CmdCnf
. (BooleanType)result = TRUE
. (IA5StringType)resultString[0] = ""
- Constraint:
ca_MMI_CmdCnf
- BinaryMessage:
80

- No.: 810
- Timestamp: 17:11:15:041_0
- RFN: 4276
- Chip: 21760
- Event: Receive
- PCO: TM
- Message: RLC_TR_DATA_IND
- Source: ts_RRC_ConnEst:lt_RcvConnReq LINE 2
- Message Structure:
RLC_TR_DATA_IND
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 0
. tM_message
. . UL_CCCH_Message
. . . IntegrityCheckInfo
. . . UL_CCCH_MessageType
. . . . RRCConnectionRequest
. . . . . InitialUE_Identity
. . . . . . IMSI_GSM_MAP
. . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . (IntegerType)_elem[4] = 1
. . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . (IntegerType)_elem[4] = 1
. . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . (IntegerType)_elem[4] = 1
. . . . . . . (IntegerType)_elem[4] = 2
. . . . . . . (IntegerType)_elem[4] = 3
. . . . . . . (IntegerType)_elem[4] = 4
. . . . . . . (IntegerType)_elem[4] = 5
. . . . . . . (IntegerType)_elem[4] = 6
. . . . . . . (IntegerType)_elem[4] = 7
. . . . . . . (IntegerType)_elem[4] = 8
. . . . . . . (IntegerType)_elem[4] = 9
. . . . . (EstablishmentCause)establishmentCause[5] = 12
. . . . . (ProtocolErrorIndicator)protocolErrorIndicator[1] = 0
. . . . . MeasuredResultsOnRACH
. . . . . v3d0NonCriticalExtensions
- Constraint:
car_RRC_ConnReq
- BinaryMessage:
30 10 02 01 00 02 01 00 20 90 01 01 01 23 45 67 89 60

- No.: 814
- Timestamp: 17:11:15:051_0
- RFN: 4277
- Chip: 23552
- Event: Send
- PCO: UM
- Message: RLC_UM_DATA_REQ
- Source: ts_RRC_ConnEst:lt_Send_ConnSetUp LINE 22
- Message Structure:
RLC_UM_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 0
. uM_message
. . DL_CCCH_Message
. . . IntegrityCheckInfo
. . . DL_CCCH_MessageType
. . . . RRCConnectionSetup
. . . . . r3
. . . . . . RRCConnectionSetup_r3_IEs
. . . . . . . InitialUE_Identity
. . . . . . . . IMSI_GSM_MAP
. . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . (IntegerType)_elem[4] = 1
. . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . (IntegerType)_elem[4] = 1
. . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . (IntegerType)_elem[4] = 1
. . . . . . . . . (IntegerType)_elem[4] = 2
. . . . . . . . . (IntegerType)_elem[4] = 3
. . . . . . . . . (IntegerType)_elem[4] = 4
. . . . . . . . . (IntegerType)_elem[4] = 5
. . . . . . . . . (IntegerType)_elem[4] = 6
. . . . . . . . . (IntegerType)_elem[4] = 7
. . . . . . . . . (IntegerType)_elem[4] = 8
. . . . . . . . . (IntegerType)_elem[4] = 9
. . . . . . . (IntegerType)rrc_TransactionIdentifier[-1] = 0
. . . . . . . (IntegerType)activationTime[-1] = -
. . . . . . . U_RNTI
. . . . . . . . (BitStringType)srnc_Identity[12] = "000000000001"
. . . . . . . . (BitStringType)s_RNTI[20] = "00000000000000000001"
. . . . . . . (BitStringType)new_c_RNTI[16] = -
. . . . . . . (RRC_StateIndicator)rrc_StateIndicator[0] = 0
. . . . . . . (IntegerType)utran_DRX_CycleLengthCoeff[-1] = 9
. . . . . . . CapabilityUpdateRequirement
. . . . . . . . (BooleanType)ue_RadioCapabilityFDDUpdateRequirement = TRUE
. . . . . . . . (BooleanType)ue_RadioCapabilityTDDUpdateRequirement = FALSE
. . . . . . . . SystemSpecificCapUpdateReqList
. . . . . . . . . (SystemSpecificCapUpdateReq)_elem[0] = 0
. . . . . . . SRB_InformationSetupList2
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity[-1] = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_UM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 1
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex[-1] = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 1
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity[-1] = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 2
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 2
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 2
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 2
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex[-1] = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 2
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 2
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity[-1] = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 3
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 3
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 3
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 3
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex[-1] = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 3
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 3
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity[-1] = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 4
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 4
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 4
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 4
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex[-1] = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 4
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 4
. . . . . . . UL_CommonTransChInfo
. . . . . . . . TFC_Subset
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . TFCS
. . . . . . . . . . . ExplicitTFCS_Configuration
. . . . . . . . . . . . TFCS_ReconfAdd
. . . . . . . . . . . . . ctfcSize
. . . . . . . . . . . . . . ctfc2Bit
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . . . . . . . (IntegerType)ctfc2[-1] = 0
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . . . . . . . (IntegerType)ctfc2[-1] = 1
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC[-1] = 11
. . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaD[-1] = 15
. . . . . . . . . . . . . . . . . . . (IntegerType)referenceTFC_ID[-1] = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . UL_AddReconfTransChInfoList
. . . . . . . . UL_AddReconfTransChInformation
. . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType[0] = 0
. . . . . . . . . (IntegerType)transportChannelIdentity[-1] = 5
. . . . . . . . . TransportFormatSet
. . . . . . . . . . DedicatedTransChTFS
. . . . . . . . . . . tti
. . . . . . . . . . . . DedicatedDynamicTF_InfoList
. . . . . . . . . . . . . DedicatedDynamicTF_Info
. . . . . . . . . . . . . . rlc_Size
. . . . . . . . . . . . . . . BitModeRLC_SizeInfo
. . . . . . . . . . . . . . . . sizeType2
. . . . . . . . . . . . . . . . . (IntegerType)part1[-1] = 2
. . . . . . . . . . . . . . . . . (IntegerType)part2[-1] = -
. . . . . . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . LogicalChannelList
. . . . . . . . . . . SemistaticTF_Information
. . . . . . . . . . . . ChannelCodingType
. . . . . . . . . . . . . (CodingRate)convolutional[0] = 1
. . . . . . . . . . . . (IntegerType)rateMatchingAttribute[-1] = 192
. . . . . . . . . . . . (CRC_Size)crc_Size[0] = 3
. . . . . . . DL_CommonTransChInfo
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . dl_Parameters
. . . . . . . DL_AddReconfTransChInfoList
. . . . . . . . DL_AddReconfTransChInformation
. . . . . . . . . (DL_TrCH_Type)dl_TransportChannelType[0] = 0
. . . . . . . . . (IntegerType)dl_transportChannelIdentity[-1] = 10
. . . . . . . . . tfs_SignallingMode
. . . . . . . . . . UL_TransportChannelIdentity
. . . . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType[0] = 0
. . . . . . . . . . . (IntegerType)ul_TransportChannelIdentity[-1] = 5
. . . . . . . . . QualityTarget
. . . . . . . . . . (IntegerType)bler_QualityValue[-1] = -20
. . . . . . . . . TM_SignallingInfo
. . . . . . . FrequencyInfo
. . . . . . . (IntegerType)maxAllowedUL_TX_Power[-1] = -
. . . . . . . UL_ChannelRequirement
. . . . . . . . UL_DPCH_Info
. . . . . . . . . UL_DPCH_PowerControlInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (IntegerType)dpcch_PowerOffset[-1] = -40
. . . . . . . . . . . (IntegerType)pc_Preamble[-1] = 1
. . . . . . . . . . . (IntegerType)sRB_delay[-1] = 7
. . . . . . . . . . . PowerControlAlgorithm
. . . . . . . . . . . . (IntegerType)algorithm1[-1] = 1
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (ScramblingCodeType)scramblingCodeType[0] = 1
. . . . . . . . . . . (IntegerType)scramblingCode[-1] = 0
. . . . . . . . . . . (IntegerType)numberOfDPDCH[-1] = -
. . . . . . . . . . . (SpreadingFactor)spreadingFactor[0] = 4
. . . . . . . . . . . (BooleanType)tfci_Existence = TRUE
. . . . . . . . . . . (IntegerType)numberOfFBI_Bits[-1] = -
. . . . . . . . . . . (PuncturingLimit)puncturingLimit[0] = 15
. . . . . . . DL_CommonInformation
. . . . . . . . DL_DPCH_InfoCommon
. . . . . . . . . cfnHandling
. . . . . . . . . . initialise
. . . . . . . . . . . (IntegerType)cfntargetsfnframeoffset[-1] = -
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . DL_DPCH_PowerControlInfo
. . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . (DPC_Mode)dpc_Mode[0] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPilot_pdpdch[-1] = 0
. . . . . . . . . . . Dl_rate_matching_restriction
. . . . . . . . . . . SF512_AndPilot
. . . . . . . . . . . . (PilotBits128)sfd128[0] = 0
. . . . . . . . . . . (PositionFixedOrFlexible)positionFixedOrFlexible[0] = 0
. . . . . . . . . . . (BooleanType)tfci_Existence = FALSE
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . (IntegerType)defaultDPCH_OffsetValue[-1] = 459
. . . . . . . . . . DPCH_CompressedModeInfo
. . . . . . . . . . (TX_DiversityMode)tx_DiversityMode[0] = 0
. . . . . . . . . . SSDT_Information
. . . . . . . DL_InformationPerRL_List
. . . . . . . . DL_InformationPerRL
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . PrimaryCPICH_Info
. . . . . . . . . . . . (IntegerType)primaryScramblingCode[-1] = 100
. . . . . . . . . . . PDSCH_SHO_DCH_Info
. . . . . . . . . . . PDSCH_CodeMapping
. . . . . . . . . DL_DPCH_InfoPerRL
. . . . . . . . . . fdd
. . . . . . . . . . . (PCPICH_UsageForChannelEst)pCPICH_UsageForChannelEst[0] = 0
. . . . . . . . . . . (IntegerType)dpch_FrameOffset[-1] = 18
. . . . . . . . . . . SecondaryCPICH_Info
. . . . . . . . . . . DL_ChannelisationCodeList
. . . . . . . . . . . . DL_ChannelisationCode
. . . . . . . . . . . . . (IntegerType)secondaryScramblingCode[-1] = 1
. . . . . . . . . . . . . SF512_AndCodeNumber
. . . . . . . . . . . . . . (IntegerType)sf128[-1] = 0
. . . . . . . . . . . . . (ScramblingCodeChange)scramblingCodeChange[0] = 1
. . . . . . . . . . . (IntegerType)tpc_CombinationIndex[-1] = 0
. . . . . . . . . . . (SSDT_CellIdentity)ssdt_CellIdentity[0] = -
. . . . . . . . . . . (ClosedLoopTimingAdjMode)closedLoopTimingAdjMode[0] = -
. . . . . . . . . SCCPCH_InfoForFACH
. . . . . . laterNonCriticalExtensions
. (BooleanType)specialLI = TRUE
- Constraint:
cas_RRC_ConnSetup
- BinaryMessage:
30 78 02 01 00 02 01 00 30 e7 12 00 20 20 24 68 ac f1 20 00 80 00 09 b0 4d 27 42 02 11 21 a8 40 00 50 33 d1 c8 d9 34 cf 93 89 ce 84 14 a2 47 51 80 02 a2 67 a3 91 b2 69 9f 27 13 9d 08 4a 44 96 a5 00 09 48 cf 47 23 64 d3 3e 4e 27 3a 10 d6 89 3d 4e 00 1a 99 00 00 c4 a5 7e 00 40 01 10 44 77 ec c1 13 12 b4 a8 f4 40 00 00 27 f2 01 42 9c b0 40 c8 01 21 85 01 00 01 01 ff

- No.: 835
- Timestamp: 17:11:15:074_2
- RFN: 4279
- Chip: 33536
- Event: Start Timer
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 3
- Message Structure:
no details available
- Constraint:
t_WaitMS (13500 Ms)
- BinaryMessage:

- No.: 842
- Timestamp: 17:11:15:273_1
- RFN: 4299
- Chip: 29184
- Event: Receive
- PCO: CPHY
- Message: CPHY_Sync_IND
- Source: RRC_DefConnEst LINE 5
- Message Structure:
CPHY_Sync_IND
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 20
- Constraint:
ca_SyncInd
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 844
- Timestamp: 17:11:15:274_0
- RFN: 4299
- Chip: 30976
- Event: Default
- Source: RRC_DefConnEst LINE 0
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 845
- Timestamp: 17:11:15:274_1
- RFN: 4299
- Chip: 31232
- Event: Default
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 852
- Timestamp: 17:11:15:395_0
- RFN: 4312
- Chip: 0
- Event: Receive
- PCO: AM
- Message: RLC_AM_DATA_IND
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
RLC_AM_DATA_IND
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 2
. IntegrityResult
. . (IntegrityStatus)integrityUsed[0] = 4294967296
. aM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . UL_DCCH_MessageType
. . . . RRCConnectionSetupComplete
. . . . . (IntegerType)rrc_TransactionIdentifier[2] = 0
. . . . . STARTList
. . . . . . STARTSingle
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity[1] = 0
. . . . . . . (BitStringType)start_Value[20] = "11111111111111111111"
. . . . . . STARTSingle
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity[1] = 1
. . . . . . . (BitStringType)start_Value[20] = "00000000000000000010"
. . . . . UE_RadioAccessCapability
. . . . . . (AccessStratumReleaseIndicator)accessStratumReleaseIndicator[0] = 0
. . . . . . PDCP_Capability
. . . . . . . (BooleanType)losslessSRNS_RelocationSupport = TRUE
. . . . . . . supportForRfc2507
. . . . . . RLC_Capability
. . . . . . . (TotalRLC_AM_BufferSize)totalRLC_AM_BufferSize[3] = 2
. . . . . . . (MaximumRLC_WindowSize)maximumRLC_WindowSize[1] = 0
. . . . . . . (MaximumAM_EntityNumberRLC_Cap)maximumAM_EntityNumber[3] = 3
. . . . . . TransportChannelCapability
. . . . . . . DL_TransChCapability
. . . . . . . . (MaxNoBits)maxNoBitsReceived[4] = 4
. . . . . . . . (MaxNoBits)maxConvCodeBitsReceived[4] = 0
. . . . . . . . TurboSupport
. . . . . . . . . (MaxNoBits)supported[4] = 4
. . . . . . . . (MaxSimultaneousTransChsDL)maxSimultaneousTransChs[2] = 1
. . . . . . . . (IntegerType)maxSimultaneousCCTrCH_Count[3] = 1
. . . . . . . . (MaxTransportBlocksDL)maxReceivedTransportBlocks[4] = 3
. . . . . . . . (MaxNumberOfTFC_DL)maxNumberOfTFC[4] = 5
. . . . . . . . (MaxNumberOfTF)maxNumberOfTF[3] = 1
. . . . . . . UL_TransChCapability
. . . . . . . . (MaxNoBits)maxNoBitsTransmitted[4] = 3
. . . . . . . . (MaxNoBits)maxConvCodeBitsTransmitted[4] = 0
. . . . . . . . TurboSupport
. . . . . . . . . (MaxNoBits)supported[4] = 3
. . . . . . . . (MaxSimultaneousTransChsUL)maxSimultaneousTransChs[3] = 2
. . . . . . . . modeSpecificInfo
. . . . . . . . (MaxTransportBlocksUL)maxTransmittedBlocks[4] = 2
. . . . . . . . (MaxNumberOfTFC_UL)maxNumberOfTFC[4] = 3
. . . . . . . . (MaxNumberOfTF)maxNumberOfTF[3] = 0
. . . . . . RF_Capability
. . . . . . . fddRF_Capability
. . . . . . . tddRF_Capability
. . . . . . PhysicalChannelCapability
. . . . . . . fddPhysChCapability
. . . . . . . . DL_PhysChCapabilityFDD
. . . . . . . . . (IntegerType)maxNoDPCH_PDSCH_Codes[3] = 3
. . . . . . . . . (MaxNoPhysChBitsReceived)maxNoPhysChBitsReceived[4] = 6
. . . . . . . . . (BooleanType)supportForSF_512 = FALSE
. . . . . . . . . (BooleanType)supportOfPDSCH = FALSE
. . . . . . . . . SimultaneousSCCPCH_DPCH_Reception
. . . . . . . . UL_PhysChCapabilityFDD
. . . . . . . . . (MaxNoDPDCH_BitsTransmitted)maxNoDPDCH_BitsTransmitted[4] = 2
. . . . . . . . . (BooleanType)supportOfPCPCH = FALSE
. . . . . . . tddPhysChCapability
. . . . . . UE_MultiModeRAT_Capability
. . . . . . . MultiRAT_Capability
. . . . . . . . (BooleanType)supportOfGSM = FALSE
. . . . . . . . (BooleanType)supportOfMulticarrier = FALSE
. . . . . . . (MultiModeCapability)multiModeCapability[2] = 1
. . . . . . SecurityCapability
. . . . . . . (BitStringType)cipheringAlgorithmCap[16] = '0000000000000001'B
. . . . . . . (BitStringType)integrityProtectionAlgorithmCap[16] = '0000000000000010'B
. . . . . . UE_Positioning_Capability
. . . . . . . (BooleanType)standaloneLocMethodsSupported = FALSE
. . . . . . . (BooleanType)ue_BasedOTDOA_Supported = FALSE
. . . . . . . (NetworkAssistedGPS_Supported)networkAssistedGPS_Supported[2] = 1
. . . . . . . (BooleanType)supportForUE_GPS_TimingOfCellFrames = FALSE
. . . . . . . (BooleanType)supportForIPDL = FALSE
. . . . . . MeasurementCapability
. . . . . v370NonCriticalExtensions
. . . . . . RRCConnectionSetupComplete_v370ext
. . . . . . . UE_RadioAccessCapability_v370ext
. . . . . . . . UE_RadioAccessCapabBandFDDList
. . . . . . . . . UE_RadioAccessCapabBandFDD
. . . . . . . . . . (RadioFrequencyBandFDD)radioFrequencyBandFDD[3] = 1
. . . . . . . . . . fddRF_Capability
. . . . . . . . . . . (UE_PowerClassExt)ue_PowerClass[3] = 3
. . . . . . . . . . . (TxRxFrequencySeparation)txRxFrequencySeparation[2] = 0
. . . . . . . . . . MeasurementCapabilityExt
. . . . . . . . . . . CompressedModeMeasCapabFDDList
. . . . . . . . . . . . CompressedModeMeasCapabFDD
. . . . . . . . . . . . . (RadioFrequencyBandFDD)radioFrequencyBandFDD[3] = 1
. . . . . . . . . . . . . (BooleanType)dl_MeasurementsFDD = TRUE
. . . . . . . . . . . . . (BooleanType)ul_MeasurementsFDD = TRUE
. . . . . . . . . . . CompressedModeMeasCapabGSMList
. . . . . . . . . . . . CompressedModeMeasCapabGSM
. . . . . . . . . . . . . (RadioFrequencyBandGSM)radioFrequencyBandGSM[4] = 2
. . . . . . . . . . . . . (BooleanType)dl_MeasurementsGSM = FALSE
. . . . . . . . . . . . . (BooleanType)ul_MeasurementsGSM = FALSE
. . . . . . . . . . . . CompressedModeMeasCapabGSM
. . . . . . . . . . . . . (RadioFrequencyBandGSM)radioFrequencyBandGSM[4] = 6
. . . . . . . . . . . . . (BooleanType)dl_MeasurementsGSM = FALSE
. . . . . . . . . . . . . (BooleanType)ul_MeasurementsGSM = TRUE
. . . . . . . . . . . CompressedModeMeasCapabMC
. . . . . . v380NonCriticalExtensions
- Constraint:
car_RRC_ConnSetupCmpl
- BinaryMessage:
30 2a 02 01 ff 02 01 02 0a 05 01 00 00 00 00 4a 8b ff ff e0 00 04 91 a0 51 06 a4 c2 68 46 09 30 20 80 00 80 01 08 89 62 13 89 0c 80

- No.: 854
- Timestamp: 17:11:15:397_1
- RFN: 4312
- Chip: 8448
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 876
- Timestamp: 17:11:15:534_0
- RFN: 4325
- Chip: 33280
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_GMM_IdleUpdated:lt_AttachRequest LINE 1
- Message Structure:
RRC_DataInd
. (IntegerType)cellId[0] = -1
. (SS_RB_Identity)rB_Id[0] = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain[0] = 1
. (START_Value)start[20] = '00000000000000000010'B
. ATTACHREQUEST
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)gMMProtocolDiscriminator[4] = '1000'B
. . (MsgType)msgType[8] = '00000001'B
. . MS_NetworkCap_lv
. . . (Length)iel[1] = '02'O
. . . (OctetStringType)value[2] = 'C500'O
. . CiphKeySeqNum
. . . (B1)spare1[1] = '0'B
. . . (KeySeq)keySeq[3] = '111'B
. . AttachType
. . . (B1)pre_for[1] = '0'B
. . . (B3)type[3] = '011'B
. . DRXparamter
. . . (B8)splitPGcycleCode[8] = '00001101'B
. . . (B4)cnDRXcoef[4] = '0000'B
. . . (B1)splitOnCCCH[1] = '0'B
. . . (B3)nonDRXtimer[3] = '011'B
. . MS_Identity_lv
. . . (Length)iel[1] = '08'O
. . . (B4)iDigit1[4] = '0000'B
. . . (B1)oddEvenInd[1] = '1'B
. . . (B3)typeOfId[3] = '001'B
. . . (OctetStringType)otherDigits[7] = '10101032547698'O
. . RAI_v
. . . (OctetStringType)plmn[3] = '00F110'O
. . . (OctetStringType)lac[2] = 'FFFE'O
. . . (OctetStringType)rac[1] = '05'O
. . MSRadioAccessCap_lv
. . . (Length)iel[1] = '05'O
. . . (OctetStringType)value[5] = '02C2000600'O
. . PTMSI_Signature
. . GPRS_Timer
. . TMSI_Status
. . . (IEI4)iei[4] = '1001'B
. . . (B3)spare3[3] = '000'B
. . . (B1)flag[1] = '0'B
- Constraint:
car_PS_InitDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 03 04 04 00 00 20 08 01 02 c5 00 73 0d 03 08 09 10 10 10 32 54 76 98 00 f1 10 ff fe 05 05 02 c2 00 06 00 90

- No.: 913
- Timestamp: 17:11:15:541_0
- RFN: 4326
- Chip: 18944
- Event: Send
- PCO: Dc
- Message: RRC_DataReq
- Source: ts_GMM_Authentication LINE 2
- Message Structure:
RRC_DataReq
. (IntegerType)cellId[-1] = -1
. (SS_RB_Identity)rB_Id[-1] = 3
. (LogicChGERAN)ch[-1] = -
. (SapId)sapId[1] = -
. (SS_CN_DomainIdentity)cN_Domain[-1] = 1
. AUTHENTICATIONANDCIPHERINGREQUEST
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)gMMProtocolDiscriminator[4] = '1000'B
. . (MsgType)msgType[8] = '00010010'B
. . IMEISVRequest
. . . (B1)spare1[1] = '0'B
. . . (B3)value[3] = '000'B
. . CiphAlgorithm
. . . (B1)spare1[1] = '0'B
. . . (B3)algorithm[3] = '001'B
. . AC_ReferenceNumber
. . . (B4)value[4] = '0011'B
. . ForceToStandby
. . . (B1)spare[1] = '0'B
. . . (B3)value[3] = '000'B
. . AuthenticationParamterRAND
. . . (IEI8)iei[8] = '00100001'B
. . . (BitStringType)randValue[128] = '01010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101'B
. . CiphKeySeqNum_tv
. . . (IEI4)iei[4] = '1000'B
. . . (B1)spare1[1] = '0'B
. . . (KeySeq)keySeq[3] = '000'B
. . GMM_AUTN
. . . (IEI8)iei[8] = '00101000'B
. . . (Length)iel[1] = '10'O
. . . (BitStringType)aUTN[128] = '01100110000100010000000000110011001000101101110100000000000000000101010101000100011101110110011000010001000000000011001100100010'B
- Constraint:
ca_PS_DataReq
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 08 12 01 30 21 55 55 55 55 55 55 55 55 55 55 55 55 55 55 55 55 80 28 10 66 11 00 33 22 dd 00 00 55 44 77 66 11 00 33 22

- No.: 917
- Timestamp: 17:11:15:893_0
- RFN: 4361
- Chip: 30464
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_GMM_Authentication LINE 3
- Message Structure:
RRC_DataInd
. (IntegerType)cellId[0] = -1
. (SS_RB_Identity)rB_Id[0] = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain[0] = 1
. (START_Value)start[0] = -
. AUTHENTICATIONANDCIPHERINGRESPONSE
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)gMMProtocolDiscriminator[4] = '1000'B
. . (MsgType)msgType[8] = '00010011'B
. . (B4)spare4[4] = '0000'B
. . AC_ReferenceNumber
. . . (B4)value[4] = '0011'B
. . AuthRsp_tv
. . . (IEI8)iei[8] = '00100010'B
. . . (BitStringType)value[32] = '01010101010001000111011101100110'B
. . GMM_MS_Identity
. . AuthRspExt
. . . (IEI8)iei[8] = '00101001'B
. . . (Length)iel[1] = '04'O
. . . (BitStringType)rES[32] = '00010001000000000011001100100010'B
- Constraint:
car_PS_UplinkDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 08 13 03 22 55 44 77 66 29 04 11 00 33 22

- No.: 920
- Timestamp: 17:11:15:894_2
- RFN: 4361
- Chip: 33024
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_GMM_Authentication LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 982
- Timestamp: 17:11:15:902_2
- RFN: 4362
- Chip: 25856
- Event: Send
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_REQ
- Source: ts_SS_DownloadSecurityKey:lt_DownloadKeyCRLC LINE 1
- Message Structure:
CRLC_SecurityMode_Config_REQ
. (IntegerType)cellId[-1] = -1
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity[0] = 1
. . (BitStringType)startValue[20] = "00000000000000000000"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = '01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100'B
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CRLC_SecurityModeCfgReq
- BinaryMessage:
30 21 02 01 ff 30 1c 0a 01 01 03 04 04 00 00 00 03 11 00 77 66 11 00 33 22 dd cc ff ee 99 88 bb aa 55 44

- No.: 983
- Timestamp: 17:11:15:903_0
- RFN: 4362
- Chip: 27904
- Event: Receive
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_CNF
- Source: ts_SS_DownloadSecurityKey:lt_DownloadKeyCRLC LINE 2
- Message Structure:
CRLC_SecurityMode_Config_CNF
. (IntegerType)cellId[0] = -1
- Constraint:
ca_CRLC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 990
- Timestamp: 17:11:15:904_0
- RFN: 4362
- Chip: 32512
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 1
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 0
. (IntegerType)count_I_LSB_UL[-1] = -
. (IntegerType)count_I_LSB_DL[-1] = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 00 02 01 00 02 01 00

- No.: 991
- Timestamp: 17:11:15:904_1
- RFN: 4362
- Chip: 34304
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 2
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 0
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 00 02 01 00

- No.: 992
- Timestamp: 17:11:15:905_0
- RFN: 4362
- Chip: 35840
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 3
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 1
. (IntegerType)count_I_LSB_UL[-1] = -
. (IntegerType)count_I_LSB_DL[-1] = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 01 02 01 00

- No.: 993
- Timestamp: 17:11:15:905_1
- RFN: 4362
- Chip: 37632
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 4
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 1
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 994
- Timestamp: 17:11:15:906_0
- RFN: 4363
- Chip: 1792
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 5
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 2
. (IntegerType)count_I_LSB_UL[-1] = -
. (IntegerType)count_I_LSB_DL[-1] = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 02 02 01 00

- No.: 995
- Timestamp: 17:11:15:906_1
- RFN: 4363
- Chip: 3328
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 6
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 2
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 996
- Timestamp: 17:11:15:907_0
- RFN: 4363
- Chip: 5120
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 7
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 3
. (IntegerType)count_I_LSB_UL[-1] = -
. (IntegerType)count_I_LSB_DL[-1] = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 03 02 01 00

- No.: 997
- Timestamp: 17:11:15:907_1
- RFN: 4363
- Chip: 6656
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 8
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 3
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 998
- Timestamp: 17:11:15:908_0
- RFN: 4363
- Chip: 8448
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 9
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 4
. (IntegerType)count_I_LSB_UL[-1] = -
. (IntegerType)count_I_LSB_DL[-1] = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 04 02 01 00

- No.: 999
- Timestamp: 17:11:15:908_1
- RFN: 4363
- Chip: 9984
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 10
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 4
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 1003
- Timestamp: 17:11:15:909_1
- RFN: 4363
- Chip: 14080
- Event: Send
- PCO: CRLC
- Message: CRLC_Integrity_Activate_REQ
- Source: ts_CRLC_DL_Integrity LINE 1
- Message Structure:
CRLC_Integrity_Activate_REQ
. (IntegerType)cellId[-1] = -1
. (CN_DomainIdentity)cn_DomainIdentity[0] = 1
. IntegrityActivationInfo
. . IntegrityProtectionModeInfo
. . . IntegrityProtectionModeCommand
. . . . startIntegrityProtection
. . . . . (BitStringType)integrityProtInitNumber[32] = "00000000000000000000000000000001"
. . . (IntegrityProtectionAlgorithm)integrityProtectionAlgorithm[0] = 0
- Constraint:
ca_CRLC_DL_IntegrityActivateReq
- BinaryMessage:
30 14 02 01 ff 0a 01 01 30 0c 30 07 03 05 00 00 00 00 01 0a 01 00

- No.: 1004
- Timestamp: 17:11:15:910_0
- RFN: 4363
- Chip: 15872
- Event: Receive
- PCO: CRLC
- Message: CRLC_Integrity_Activate_CNF
- Source: ts_CRLC_DL_Integrity LINE 2
- Message Structure:
CRLC_Integrity_Activate_CNF
. (IntegerType)cellId[0] = -1
- Constraint:
ca_CRLC_IntegrityActivateCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1011
- Timestamp: 17:11:15:911_0
- RFN: 4363
- Chip: 20992
- Event: Send
- PCO: CRLC
- Message: CRLC_Integrity_Activate_REQ
- Source: ts_RB2_UL_IntegrityActivate LINE 1
- Message Structure:
CRLC_Integrity_Activate_REQ
. (IntegerType)cellId[-1] = -1
. (CN_DomainIdentity)cn_DomainIdentity[0] = 1
. IntegrityActivationInfo
. . IntegrityProtActivationInfoList
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity[-1] = 2
. . . . (IntegerType)rrc_MessageSequenceNumber[-1] = 0
- Constraint:
ca_CRLC_UL_IntegrityActivateReq
- BinaryMessage:
30 10 02 01 ff 0a 01 01 30 08 30 06 02 01 02 02 01 00

- No.: 1012
- Timestamp: 17:11:15:911_1
- RFN: 4363
- Chip: 23040
- Event: Receive
- PCO: CRLC
- Message: CRLC_Integrity_Activate_CNF
- Source: ts_RB2_UL_IntegrityActivate LINE 2
- Message Structure:
CRLC_Integrity_Activate_CNF
. (IntegerType)cellId[0] = -1
- Constraint:
ca_CRLC_IntegrityActivateCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1019
- Timestamp: 17:11:15:913_0
- RFN: 4363
- Chip: 30464
- Event: Send
- PCO: AM
- Message: RLC_AM_DATA_REQ
- Source: ts_RRC_Security:lt_SendSecurityModeCommand LINE 8
- Message Structure:
RLC_AM_DATA_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 2
. AmConfirmationRequest
. aM_message
. . DL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00000000000000000000000000000000"
. . . . (IntegerType)rrc_MessageSequenceNumber[-1] = 0
. . . DL_DCCH_MessageType
. . . . SecurityModeCommand
. . . . . r3
. . . . . . SecurityModeCommand_r3_IEs
. . . . . . . (IntegerType)rrc_TransactionIdentifier[-1] = 0
. . . . . . . SecurityCapability
. . . . . . . . (BitStringType)cipheringAlgorithmCap[16] = '0000000000000001'B
. . . . . . . . (BitStringType)integrityProtectionAlgorithmCap[16] = '0000000000000010'B
. . . . . . . CipheringModeInfo
. . . . . . . IntegrityProtectionModeInfo
. . . . . . . . IntegrityProtectionModeCommand
. . . . . . . . . startIntegrityProtection
. . . . . . . . . . (BitStringType)integrityProtInitNumber[32] = "00000000000000000000000000000001"
. . . . . . . . (IntegrityProtectionAlgorithm)integrityProtectionAlgorithm[0] = 0
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity[0] = 1
. . . . . . . InterRAT_UE_SecurityCapList
. . . . . . . . InterRAT_UE_SecurityCapability
. . . . . . . . . gsm
. . . . . . . . . . (BitStringType)gsmSecurityCapability[7] = "0000000"
. . . . . . laterNonCriticalExtensions
- Constraint:
cas_RRC_SecModeCmd
- BinaryMessage:
30 18 02 01 ff 02 01 02 05 00 80 00 00 00 04 06 00 00 80 01 40 00 00 00 30 00

- No.: 1028
- Timestamp: 17:11:16:053_0
- RFN: 4377
- Chip: 31232
- Event: Receive
- PCO: AM
- Message: RLC_AM_DATA_IND
- Source: ts_RRC_Security:lt_StartSecurity_UE LINE 8
- Message Structure:
RLC_AM_DATA_IND
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 2
. IntegrityResult
. . (IntegrityStatus)integrityUsed[0] = 0
. aM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "01100100010100101000000110010100"
. . . . (IntegerType)rrc_MessageSequenceNumber[4] = 1
. . . UL_DCCH_MessageType
. . . . SecurityModeComplete
. . . . . (IntegerType)rrc_TransactionIdentifier[2] = 0
. . . . . IntegrityProtActivationInfo
. . . . . . RRC_MessageSequenceNumberList
. . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . (IntegerType)_elem[4] = 0
. . . . . laterNonCriticalExtensions
- Constraint:
car_RRC_SecModeCmpl
- BinaryMessage:
30 12 02 01 ff 02 01 02 0a 01 00 b2 29 40 ca 0d 21 00 00 00

- No.: 1029
- Timestamp: 17:11:16:053_1
- RFN: 4377
- Chip: 32768
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_Security:lt_StartSecurity_UE LINE 8
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1031
- Timestamp: 17:11:16:054_1
- RFN: 4377
- Chip: 35584
- Event: Send
- PCO: CRLC
- Message: CRLC_Integrity_Activate_REQ
- Source: ts_CRLC_UL_Integrity LINE 1
- Message Structure:
CRLC_Integrity_Activate_REQ
. (IntegerType)cellId[-1] = -1
. (CN_DomainIdentity)cn_DomainIdentity[0] = 1
. IntegrityActivationInfo
. . IntegrityProtActivationInfoList
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity[-1] = 0
. . . . (IntegerType)rrc_MessageSequenceNumber[-1] = 0
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity[-1] = 1
. . . . (IntegerType)rrc_MessageSequenceNumber[-1] = 0
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity[-1] = 3
. . . . (IntegerType)rrc_MessageSequenceNumber[-1] = 0
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity[-1] = 4
. . . . (IntegerType)rrc_MessageSequenceNumber[-1] = 0
- Constraint:
ca_CRLC_UL_IntegrityActivateReq
- BinaryMessage:
30 28 02 01 ff 0a 01 01 30 20 30 06 02 01 00 02 01 00 30 06 02 01 01 02 01 00 30 06 02 01 03 02 01 00 30 06 02 01 04 02 01 00

- No.: 1032
- Timestamp: 17:11:16:055_0
- RFN: 4377
- Chip: 37632
- Event: Receive
- PCO: CRLC
- Message: CRLC_Integrity_Activate_CNF
- Source: ts_CRLC_UL_Integrity LINE 2
- Message Structure:
CRLC_Integrity_Activate_CNF
. (IntegerType)cellId[0] = -1
- Constraint:
ca_CRLC_IntegrityActivateCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1042
- Timestamp: 17:11:16:057_0
- RFN: 4378
- Chip: 7936
- Event: Send
- PCO: Dc
- Message: RRC_DataReq
- Source: ts_GMM_IdleUpdated:lt_AttachAccept LINE 4
- Message Structure:
RRC_DataReq
. (IntegerType)cellId[-1] = -1
. (SS_RB_Identity)rB_Id[-1] = 3
. (LogicChGERAN)ch[-1] = -
. (SapId)sapId[1] = -
. (SS_CN_DomainIdentity)cN_Domain[-1] = 1
. ATTACHACCEPT
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)gMMProtocolDiscriminator[4] = '1000'B
. . (MsgType)msgType[8] = '00000010'B
. . ForceToStandby
. . . (B1)spare[1] = '0'B
. . . (B3)value[3] = '000'B
. . AttachResult
. . . (B1)spare[1] = '0'B
. . . (B3)result[3] = '011'B
. . GPRS_Timer_v
. . . (B3)unit[3] = '111'B
. . . (B5)value[5] = '00000'B
. . (B4)spare[4] = '0000'B
. . RadioPriority_v
. . . (B1)spare[1] = '0'B
. . . (B3)value[3] = '100'B
. . RAI_v
. . . (OctetStringType)plmn[3] = '00F110'O
. . . (OctetStringType)lac[2] = '0001'O
. . . (OctetStringType)rac[1] = '05'O
. . PTMSI_Signature
. . . (IEI8)iei[8] = '00011001'B
. . . (OctetStringType)value[3] = 'AB1234'O
. . GPRS_Timer
. . GMM_MS_IdentityPTMSI
. . . (IEI8)iei[8] = '00011000'B
. . . (Length)iel[1] = '05'O
. . . (B4)iDigit1[4] = '1111'B
. . . (B1)oddEvenInd[1] = '0'B
. . . (B3)typeOfId[3] = '100'B
. . . (OctetStringType)otherDigits[-1] = '12345678'O
. . GMM_MS_Identity
. . . (IEI8)iei[8] = '00100011'B
. . . (Length)iel[1] = '05'O
. . . (B4)iDigit1[4] = '1111'B
. . . (B1)oddEvenInd[1] = '0'B
. . . (B3)typeOfId[3] = '100'B
. . . (OctetStringType)otherDigits[-1] = '12345678'O
. . GMM_Cause
. . GPRS_Timer
. . CellNotification
. . PLMN_List
- Constraint:
ca_PS_DataReq
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 08 02 03 e0 04 00 f1 10 00 01 05 19 ab 12 34 18 05 f4 12 34 56 78 23 05 f4 12 34 56 78

- No.: 1049
- Timestamp: 17:11:16:213_0
- RFN: 4393
- Chip: 30208
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_GMM_IdleUpdated:lt_AttachAccept LINE 5
- Message Structure:
RRC_DataInd
. (IntegerType)cellId[0] = -1
. (SS_RB_Identity)rB_Id[0] = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain[0] = 1
. (START_Value)start[0] = -
. ATTACHCOMPLETE
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)gMMProtocolDiscriminator[4] = '1000'B
. . (MsgType)msgType[8] = '00000011'B
- Constraint:
car_PS_UplinkDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 08 03

- No.: 1060
- Timestamp: 17:11:16:215_2
- RFN: 4393
- Chip: 35840
- Event: Start Timer
- Source: ts_RRC_Delay LINE 1
- Message Structure:
no details available
- Constraint:
t_Dly (1000 Ms)
- BinaryMessage:

- No.: 1064
- Timestamp: 17:11:17:219_0
- RFN: 4494
- Chip: 15616
- Event: Timeout
- Source: ts_RRC_Delay LINE 2
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 1069
- Timestamp: 17:11:17:221_0
- RFN: 4494
- Chip: 21248
- Event: Send
- PCO: UM
- Message: RLC_UM_DATA_REQ
- Source: ts_RRC_ConnRel:lt_Send_RRC_ConnectionRelease LINE 3
- Message Structure:
RLC_UM_DATA_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 1
. uM_message
. . DL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00000000000000000000000000000000"
. . . . (IntegerType)rrc_MessageSequenceNumber[-1] = 0
. . . DL_DCCH_MessageType
. . . . RRCConnectionRelease
. . . . . r3
. . . . . . RRCConnectionRelease_r3_IEs
. . . . . . . (IntegerType)rrc_TransactionIdentifier[-1] = 0
. . . . . . . (IntegerType)n_308[-1] = 1
. . . . . . . (ReleaseCause)releaseCause[0] = 0
. . . . . . . Rplmn_Information
. . . . . . laterNonCriticalExtensions
. (BooleanType)specialLI = FALSE
- Constraint:
cas_RRC_ConnRelDCCH
- BinaryMessage:
30 10 02 01 ff 02 01 01 80 00 00 00 03 c8 00 01 01 00

- No.: 1073
- Timestamp: 17:11:17:342_0
- RFN: 4506
- Chip: 29184
- Event: Receive
- PCO: UM
- Message: RLC_UM_DATA_IND
- Source: ts_RRC_ConnRel:lt_Send_RRC_ConnectionRelease LINE 4
- Message Structure:
RLC_UM_DATA_IND
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 1
. IntegrityResult
. uM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00100111010100110001100010101000"
. . . . (IntegerType)rrc_MessageSequenceNumber[4] = 1
. . . UL_DCCH_MessageType
. . . . RRCConnectionReleaseComplete
. . . . . (IntegerType)rrc_TransactionIdentifier[2] = 0
. . . . . FailureCauseWithProtErr
. . . . . laterNonCriticalExtensions
- Constraint:
car_RRC_ConnRelCmplUM
- BinaryMessage:
30 0e 02 01 ff 02 01 01 05 00 93 a9 8c 54 0c 40

- No.: 1074
- Timestamp: 17:11:17:343_0
- RFN: 4506
- Chip: 30464
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ConnRel:lt_Send_RRC_ConnectionRelease LINE 4
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1077
- Timestamp: 17:11:17:343_3
- RFN: 4506
- Chip: 32256
- Event: Start Timer
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 1
- Message Structure:
no details available
- Constraint:
t_Dly (5000 Ms)
- BinaryMessage:

- No.: 1081
- Timestamp: 17:11:17:503_0
- RFN: 4522
- Chip: 28672
- Event: Receive
- PCO: UM
- Message: RLC_UM_DATA_IND
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 4
- Message Structure:
RLC_UM_DATA_IND
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 1
. IntegrityResult
. uM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "01100001101000101010011110101100"
. . . . (IntegerType)rrc_MessageSequenceNumber[4] = 2
. . . UL_DCCH_MessageType
. . . . RRCConnectionReleaseComplete
. . . . . (IntegerType)rrc_TransactionIdentifier[2] = 0
. . . . . FailureCauseWithProtErr
. . . . . laterNonCriticalExtensions
- Constraint:
car_RRC_ConnRelCmplUM
- BinaryMessage:
30 0e 02 01 ff 02 01 01 05 00 b0 d1 53 d6 14 40

- No.: 1083
- Timestamp: 17:11:17:503_2
- RFN: 4522
- Chip: 30464
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 4
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1089
- Timestamp: 17:11:17:504_3
- RFN: 4522
- Chip: 35072
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 1
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 01 0a 01 00 05 00

- No.: 1093
- Timestamp: 17:11:17:511_0
- RFN: 4523
- Chip: 22016
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 1096
- Timestamp: 17:11:17:512_0
- RFN: 4523
- Chip: 25856
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 2
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 02 0a 01 00 05 00

- No.: 1100
- Timestamp: 17:11:17:515_0
- RFN: 4524
- Chip: 256
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 1103
- Timestamp: 17:11:17:516_1
- RFN: 4524
- Chip: 3840
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 3
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 03 0a 01 00 05 00

- No.: 1107
- Timestamp: 17:11:17:522_0
- RFN: 4524
- Chip: 25088
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 3
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 1110
- Timestamp: 17:11:17:523_0
- RFN: 4524
- Chip: 28416
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 4
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 04 0a 01 00 05 00

- No.: 1114
- Timestamp: 17:11:17:530_0
- RFN: 4525
- Chip: 19200
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 4
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 1117
- Timestamp: 17:11:17:532_0
- RFN: 4525
- Chip: 25600
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 1
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 136
. . . . . UL_RLC_Mode
. . . . . . UL_UM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (NoExplicitDiscard)timerBasedNoExplicit[0] = 9
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 1
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 1
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_UM_Info
- BinaryMessage:
30 22 02 01 ff 02 01 01 0a 01 00 30 17 30 0d 05 00 30 09 02 02 00 88 30 03 0a 01 09 30 06 02 01 01 02 01 01

- No.: 1121
- Timestamp: 17:11:17:536_0
- RFN: 4526
- Chip: 2560
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 1122
- Timestamp: 17:11:17:538_0
- RFN: 4526
- Chip: 9728
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 3
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 2
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 2
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 2
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 02 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 13 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 02 02 01 02

- No.: 1126
- Timestamp: 17:11:17:550_0
- RFN: 4527
- Chip: 20736
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 4
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 1127
- Timestamp: 17:11:17:552_0
- RFN: 4527
- Chip: 27136
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 5
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 3
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 3
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 3
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 03 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 13 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 03 02 01 03

- No.: 1131
- Timestamp: 17:11:17:566_0
- RFN: 4529
- Chip: 2304
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 6
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 3
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 1132
- Timestamp: 17:11:17:567_0
- RFN: 4529
- Chip: 9216
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 7
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 4
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 4
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 4
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 04 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 13 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 04 02 01 04

- No.: 1136
- Timestamp: 17:11:17:581_0
- RFN: 4530
- Chip: 23296
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 8
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 4
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 1165
- Timestamp: 17:11:17:585_0
- RFN: 4530
- Chip: 37120
- Event: Start Timer
- Source: ts_RRC_Delay LINE 1
- Message Structure:
no details available
- Constraint:
t_Dly (5000 Ms)
- BinaryMessage:

- No.: 1170
- Timestamp: 17:11:17:641_1
- RFN: 4536
- Chip: 25088
- Event: Receive
- PCO: CPHY
- Message: CPHY_Out_of_Sync_IND
- Source: RRC_Def1 LINE 19
- Message Structure:
CPHY_Out_of_Sync_IND
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 20
- Constraint:
ca_OutOfSyncInd
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 1172
- Timestamp: 17:11:17:642_0
- RFN: 4536
- Chip: 26368
- Event: Default
- Source: RRC_Def1 LINE 0
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1173
- Timestamp: 17:11:17:642_1
- RFN: 4536
- Chip: 26880
- Event: Default
- Source: ts_RRC_Delay LINE 2
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1178
- Timestamp: 17:11:22:586_0
- RFN: 5031
- Chip: 6400
- Event: Timeout
- Source: ts_RRC_Delay LINE 2
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 1191
- Timestamp: 17:11:22:588_2
- RFN: 5031
- Chip: 13824
- Event: Send
- PCO: Ut
- Message: MMI_CmdReq
- Source: ts_MMI_UE_SwitchOff LINE 2
- Message Structure:
MMI_CmdReq
. (IA5StringType)cmd[-1] = "Please switch off the UE"
- Constraint:
ca_MMI_CmdReq
- BinaryMessage:
50 6c 65 61 73 65 20 73 77 69 74 63 68 20 6f 66 66 20 20 74 68 65 20 55 45

- No.: 1195
- Timestamp: 17:11:25:311_0
- RFN: 5303
- Chip: 23040
- Event: Receive
- PCO: Ut
- Message: MMI_CmdCnf
- Source: ts_MMI_UE_SwitchOff LINE 3
- Message Structure:
MMI_CmdCnf
. (BooleanType)result = TRUE
. (IA5StringType)resultString[0] = ""
- Constraint:
ca_MMI_CmdCnf
- BinaryMessage:
80

- No.: 1215
- Timestamp: 17:11:29:455_0
- RFN: 5718
- Chip: 2304
- Event: Receive
- PCO: TM
- Message: RLC_TR_DATA_IND
- Source: ts_RRC_ConnEst:lt_RcvConnReq LINE 4
- Message Structure:
RLC_TR_DATA_IND
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 0
. tM_message
. . UL_CCCH_Message
. . . IntegrityCheckInfo
. . . UL_CCCH_MessageType
. . . . RRCConnectionRequest
. . . . . InitialUE_Identity
. . . . . . TMSI_and_LAI_GSM_MAP
. . . . . . . (BitStringType)tmsi[32] = "00010010001101000101011001111000"
. . . . . . . LAI
. . . . . . . . PLMN_Identity
. . . . . . . . . MCC
. . . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . . (IntegerType)_elem[4] = 1
. . . . . . . . . MNC
. . . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . . (IntegerType)_elem[4] = 1
. . . . . . . . (BitStringType)lac[16] = '0000000000000001'B
. . . . . (EstablishmentCause)establishmentCause[5] = 13
. . . . . (ProtocolErrorIndicator)protocolErrorIndicator[1] = 0
. . . . . MeasuredResultsOnRACH
. . . . . v3d0NonCriticalExtensions
- Constraint:
car_RRC_ConnReq
- BinaryMessage:
30 11 02 01 00 02 01 00 21 12 34 56 78 00 10 08 00 0b 40

- No.: 1219
- Timestamp: 17:11:29:464_0
- RFN: 5719
- Chip: 1024
- Event: Send
- PCO: UM
- Message: RLC_UM_DATA_REQ
- Source: ts_RRC_ConnEst:lt_Send_ConnSetUp LINE 22
- Message Structure:
RLC_UM_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 0
. uM_message
. . DL_CCCH_Message
. . . IntegrityCheckInfo
. . . DL_CCCH_MessageType
. . . . RRCConnectionSetup
. . . . . r3
. . . . . . RRCConnectionSetup_r3_IEs
. . . . . . . InitialUE_Identity
. . . . . . . . TMSI_and_LAI_GSM_MAP
. . . . . . . . . (BitStringType)tmsi[32] = "00010010001101000101011001111000"
. . . . . . . . . LAI
. . . . . . . . . . PLMN_Identity
. . . . . . . . . . . MCC
. . . . . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . . . . (IntegerType)_elem[4] = 1
. . . . . . . . . . . MNC
. . . . . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . . . . (IntegerType)_elem[4] = 1
. . . . . . . . . . (BitStringType)lac[16] = '0000000000000001'B
. . . . . . . (IntegerType)rrc_TransactionIdentifier[-1] = 0
. . . . . . . (IntegerType)activationTime[-1] = -
. . . . . . . U_RNTI
. . . . . . . . (BitStringType)srnc_Identity[12] = "000000000001"
. . . . . . . . (BitStringType)s_RNTI[20] = "00000000000000000001"
. . . . . . . (BitStringType)new_c_RNTI[16] = -
. . . . . . . (RRC_StateIndicator)rrc_StateIndicator[0] = 0
. . . . . . . (IntegerType)utran_DRX_CycleLengthCoeff[-1] = 9
. . . . . . . CapabilityUpdateRequirement
. . . . . . . . (BooleanType)ue_RadioCapabilityFDDUpdateRequirement = TRUE
. . . . . . . . (BooleanType)ue_RadioCapabilityTDDUpdateRequirement = FALSE
. . . . . . . . SystemSpecificCapUpdateReqList
. . . . . . . . . (SystemSpecificCapUpdateReq)_elem[0] = 0
. . . . . . . SRB_InformationSetupList2
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity[-1] = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_UM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 1
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex[-1] = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 1
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity[-1] = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 2
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 2
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 2
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 2
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex[-1] = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 2
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 2
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity[-1] = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 3
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 3
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 3
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 3
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex[-1] = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 3
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 3
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity[-1] = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 4
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 4
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 4
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 4
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex[-1] = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 4
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 4
. . . . . . . UL_CommonTransChInfo
. . . . . . . . TFC_Subset
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . TFCS
. . . . . . . . . . . ExplicitTFCS_Configuration
. . . . . . . . . . . . TFCS_ReconfAdd
. . . . . . . . . . . . . ctfcSize
. . . . . . . . . . . . . . ctfc2Bit
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . . . . . . . (IntegerType)ctfc2[-1] = 0
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . . . . . . . (IntegerType)ctfc2[-1] = 1
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC[-1] = 11
. . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaD[-1] = 15
. . . . . . . . . . . . . . . . . . . (IntegerType)referenceTFC_ID[-1] = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . UL_AddReconfTransChInfoList
. . . . . . . . UL_AddReconfTransChInformation
. . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType[0] = 0
. . . . . . . . . (IntegerType)transportChannelIdentity[-1] = 5
. . . . . . . . . TransportFormatSet
. . . . . . . . . . DedicatedTransChTFS
. . . . . . . . . . . tti
. . . . . . . . . . . . DedicatedDynamicTF_InfoList
. . . . . . . . . . . . . DedicatedDynamicTF_Info
. . . . . . . . . . . . . . rlc_Size
. . . . . . . . . . . . . . . BitModeRLC_SizeInfo
. . . . . . . . . . . . . . . . sizeType2
. . . . . . . . . . . . . . . . . (IntegerType)part1[-1] = 2
. . . . . . . . . . . . . . . . . (IntegerType)part2[-1] = -
. . . . . . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . LogicalChannelList
. . . . . . . . . . . SemistaticTF_Information
. . . . . . . . . . . . ChannelCodingType
. . . . . . . . . . . . . (CodingRate)convolutional[0] = 1
. . . . . . . . . . . . (IntegerType)rateMatchingAttribute[-1] = 192
. . . . . . . . . . . . (CRC_Size)crc_Size[0] = 3
. . . . . . . DL_CommonTransChInfo
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . dl_Parameters
. . . . . . . DL_AddReconfTransChInfoList
. . . . . . . . DL_AddReconfTransChInformation
. . . . . . . . . (DL_TrCH_Type)dl_TransportChannelType[0] = 0
. . . . . . . . . (IntegerType)dl_transportChannelIdentity[-1] = 10
. . . . . . . . . tfs_SignallingMode
. . . . . . . . . . UL_TransportChannelIdentity
. . . . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType[0] = 0
. . . . . . . . . . . (IntegerType)ul_TransportChannelIdentity[-1] = 5
. . . . . . . . . QualityTarget
. . . . . . . . . . (IntegerType)bler_QualityValue[-1] = -20
. . . . . . . . . TM_SignallingInfo
. . . . . . . FrequencyInfo
. . . . . . . (IntegerType)maxAllowedUL_TX_Power[-1] = -
. . . . . . . UL_ChannelRequirement
. . . . . . . . UL_DPCH_Info
. . . . . . . . . UL_DPCH_PowerControlInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (IntegerType)dpcch_PowerOffset[-1] = -40
. . . . . . . . . . . (IntegerType)pc_Preamble[-1] = 1
. . . . . . . . . . . (IntegerType)sRB_delay[-1] = 7
. . . . . . . . . . . PowerControlAlgorithm
. . . . . . . . . . . . (IntegerType)algorithm1[-1] = 1
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (ScramblingCodeType)scramblingCodeType[0] = 1
. . . . . . . . . . . (IntegerType)scramblingCode[-1] = 0
. . . . . . . . . . . (IntegerType)numberOfDPDCH[-1] = -
. . . . . . . . . . . (SpreadingFactor)spreadingFactor[0] = 4
. . . . . . . . . . . (BooleanType)tfci_Existence = TRUE
. . . . . . . . . . . (IntegerType)numberOfFBI_Bits[-1] = -
. . . . . . . . . . . (PuncturingLimit)puncturingLimit[0] = 15
. . . . . . . DL_CommonInformation
. . . . . . . . DL_DPCH_InfoCommon
. . . . . . . . . cfnHandling
. . . . . . . . . . initialise
. . . . . . . . . . . (IntegerType)cfntargetsfnframeoffset[-1] = -
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . DL_DPCH_PowerControlInfo
. . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . (DPC_Mode)dpc_Mode[0] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPilot_pdpdch[-1] = 0
. . . . . . . . . . . Dl_rate_matching_restriction
. . . . . . . . . . . SF512_AndPilot
. . . . . . . . . . . . (PilotBits128)sfd128[0] = 0
. . . . . . . . . . . (PositionFixedOrFlexible)positionFixedOrFlexible[0] = 0
. . . . . . . . . . . (BooleanType)tfci_Existence = FALSE
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . (IntegerType)defaultDPCH_OffsetValue[-1] = 459
. . . . . . . . . . DPCH_CompressedModeInfo
. . . . . . . . . . (TX_DiversityMode)tx_DiversityMode[0] = 0
. . . . . . . . . . SSDT_Information
. . . . . . . DL_InformationPerRL_List
. . . . . . . . DL_InformationPerRL
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . PrimaryCPICH_Info
. . . . . . . . . . . . (IntegerType)primaryScramblingCode[-1] = 100
. . . . . . . . . . . PDSCH_SHO_DCH_Info
. . . . . . . . . . . PDSCH_CodeMapping
. . . . . . . . . DL_DPCH_InfoPerRL
. . . . . . . . . . fdd
. . . . . . . . . . . (PCPICH_UsageForChannelEst)pCPICH_UsageForChannelEst[0] = 0
. . . . . . . . . . . (IntegerType)dpch_FrameOffset[-1] = 18
. . . . . . . . . . . SecondaryCPICH_Info
. . . . . . . . . . . DL_ChannelisationCodeList
. . . . . . . . . . . . DL_ChannelisationCode
. . . . . . . . . . . . . (IntegerType)secondaryScramblingCode[-1] = 1
. . . . . . . . . . . . . SF512_AndCodeNumber
. . . . . . . . . . . . . . (IntegerType)sf128[-1] = 0
. . . . . . . . . . . . . (ScramblingCodeChange)scramblingCodeChange[0] = 1
. . . . . . . . . . . (IntegerType)tpc_CombinationIndex[-1] = 0
. . . . . . . . . . . (SSDT_CellIdentity)ssdt_CellIdentity[0] = -
. . . . . . . . . . . (ClosedLoopTimingAdjMode)closedLoopTimingAdjMode[0] = -
. . . . . . . . . SCCPCH_InfoForFACH
. . . . . . laterNonCriticalExtensions
. (BooleanType)specialLI = TRUE
- Constraint:
cas_RRC_ConnSetup
- BinaryMessage:
30 78 02 01 00 02 01 00 30 e7 22 46 8a cf 00 02 01 00 01 00 04 00 00 4d 82 69 3a 10 10 89 0d 42 00 02 81 9e 8e 46 c9 a6 7c 9c 4e 74 20 a5 12 3a 8c 00 15 13 3d 1c 8d 93 4c f9 38 9c e8 42 52 24 b5 28 00 4a 46 7a 39 1b 26 99 f2 71 39 d0 86 b4 49 ea 70 00 d4 c8 00 06 25 2b f0 02 00 08 82 23 bf 66 08 98 95 a5 47 a2 00 00 01 3f 90 0a 14 e5 82 06 40 09 0c 28 08 01 01 ff

- No.: 1240
- Timestamp: 17:11:29:486_7
- RFN: 5721
- Chip: 9984
- Event: Start Timer
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 3
- Message Structure:
no details available
- Constraint:
t_WaitMS (13500 Ms)
- BinaryMessage:

- No.: 1247
- Timestamp: 17:11:29:692_0
- RFN: 5741
- Chip: 28928
- Event: Receive
- PCO: CPHY
- Message: CPHY_Sync_IND
- Source: RRC_DefConnEst LINE 5
- Message Structure:
CPHY_Sync_IND
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 20
- Constraint:
ca_SyncInd
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 1249
- Timestamp: 17:11:29:692_2
- RFN: 5741
- Chip: 30464
- Event: Default
- Source: RRC_DefConnEst LINE 0
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1250
- Timestamp: 17:11:29:692_3
- RFN: 5741
- Chip: 30720
- Event: Default
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1257
- Timestamp: 17:11:29:813_0
- RFN: 5753
- Chip: 36096
- Event: Receive
- PCO: AM
- Message: RLC_AM_DATA_IND
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
RLC_AM_DATA_IND
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 2
. IntegrityResult
. . (IntegrityStatus)integrityUsed[0] = 4294967296
. aM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . UL_DCCH_MessageType
. . . . RRCConnectionSetupComplete
. . . . . (IntegerType)rrc_TransactionIdentifier[2] = 0
. . . . . STARTList
. . . . . . STARTSingle
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity[1] = 0
. . . . . . . (BitStringType)start_Value[20] = "11111111111111111111"
. . . . . . STARTSingle
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity[1] = 1
. . . . . . . (BitStringType)start_Value[20] = "00000000000000000010"
. . . . . UE_RadioAccessCapability
. . . . . . (AccessStratumReleaseIndicator)accessStratumReleaseIndicator[0] = 0
. . . . . . PDCP_Capability
. . . . . . . (BooleanType)losslessSRNS_RelocationSupport = TRUE
. . . . . . . supportForRfc2507
. . . . . . RLC_Capability
. . . . . . . (TotalRLC_AM_BufferSize)totalRLC_AM_BufferSize[3] = 2
. . . . . . . (MaximumRLC_WindowSize)maximumRLC_WindowSize[1] = 0
. . . . . . . (MaximumAM_EntityNumberRLC_Cap)maximumAM_EntityNumber[3] = 3
. . . . . . TransportChannelCapability
. . . . . . . DL_TransChCapability
. . . . . . . . (MaxNoBits)maxNoBitsReceived[4] = 4
. . . . . . . . (MaxNoBits)maxConvCodeBitsReceived[4] = 0
. . . . . . . . TurboSupport
. . . . . . . . . (MaxNoBits)supported[4] = 4
. . . . . . . . (MaxSimultaneousTransChsDL)maxSimultaneousTransChs[2] = 1
. . . . . . . . (IntegerType)maxSimultaneousCCTrCH_Count[3] = 1
. . . . . . . . (MaxTransportBlocksDL)maxReceivedTransportBlocks[4] = 3
. . . . . . . . (MaxNumberOfTFC_DL)maxNumberOfTFC[4] = 5
. . . . . . . . (MaxNumberOfTF)maxNumberOfTF[3] = 1
. . . . . . . UL_TransChCapability
. . . . . . . . (MaxNoBits)maxNoBitsTransmitted[4] = 3
. . . . . . . . (MaxNoBits)maxConvCodeBitsTransmitted[4] = 0
. . . . . . . . TurboSupport
. . . . . . . . . (MaxNoBits)supported[4] = 3
. . . . . . . . (MaxSimultaneousTransChsUL)maxSimultaneousTransChs[3] = 2
. . . . . . . . modeSpecificInfo
. . . . . . . . (MaxTransportBlocksUL)maxTransmittedBlocks[4] = 2
. . . . . . . . (MaxNumberOfTFC_UL)maxNumberOfTFC[4] = 3
. . . . . . . . (MaxNumberOfTF)maxNumberOfTF[3] = 0
. . . . . . RF_Capability
. . . . . . . fddRF_Capability
. . . . . . . tddRF_Capability
. . . . . . PhysicalChannelCapability
. . . . . . . fddPhysChCapability
. . . . . . . . DL_PhysChCapabilityFDD
. . . . . . . . . (IntegerType)maxNoDPCH_PDSCH_Codes[3] = 3
. . . . . . . . . (MaxNoPhysChBitsReceived)maxNoPhysChBitsReceived[4] = 6
. . . . . . . . . (BooleanType)supportForSF_512 = FALSE
. . . . . . . . . (BooleanType)supportOfPDSCH = FALSE
. . . . . . . . . SimultaneousSCCPCH_DPCH_Reception
. . . . . . . . UL_PhysChCapabilityFDD
. . . . . . . . . (MaxNoDPDCH_BitsTransmitted)maxNoDPDCH_BitsTransmitted[4] = 2
. . . . . . . . . (BooleanType)supportOfPCPCH = FALSE
. . . . . . . tddPhysChCapability
. . . . . . UE_MultiModeRAT_Capability
. . . . . . . MultiRAT_Capability
. . . . . . . . (BooleanType)supportOfGSM = FALSE
. . . . . . . . (BooleanType)supportOfMulticarrier = FALSE
. . . . . . . (MultiModeCapability)multiModeCapability[2] = 1
. . . . . . SecurityCapability
. . . . . . . (BitStringType)cipheringAlgorithmCap[16] = '0000000000000001'B
. . . . . . . (BitStringType)integrityProtectionAlgorithmCap[16] = '0000000000000010'B
. . . . . . UE_Positioning_Capability
. . . . . . . (BooleanType)standaloneLocMethodsSupported = FALSE
. . . . . . . (BooleanType)ue_BasedOTDOA_Supported = FALSE
. . . . . . . (NetworkAssistedGPS_Supported)networkAssistedGPS_Supported[2] = 1
. . . . . . . (BooleanType)supportForUE_GPS_TimingOfCellFrames = FALSE
. . . . . . . (BooleanType)supportForIPDL = FALSE
. . . . . . MeasurementCapability
. . . . . v370NonCriticalExtensions
. . . . . . RRCConnectionSetupComplete_v370ext
. . . . . . . UE_RadioAccessCapability_v370ext
. . . . . . . . UE_RadioAccessCapabBandFDDList
. . . . . . . . . UE_RadioAccessCapabBandFDD
. . . . . . . . . . (RadioFrequencyBandFDD)radioFrequencyBandFDD[3] = 1
. . . . . . . . . . fddRF_Capability
. . . . . . . . . . . (UE_PowerClassExt)ue_PowerClass[3] = 3
. . . . . . . . . . . (TxRxFrequencySeparation)txRxFrequencySeparation[2] = 0
. . . . . . . . . . MeasurementCapabilityExt
. . . . . . . . . . . CompressedModeMeasCapabFDDList
. . . . . . . . . . . . CompressedModeMeasCapabFDD
. . . . . . . . . . . . . (RadioFrequencyBandFDD)radioFrequencyBandFDD[3] = 1
. . . . . . . . . . . . . (BooleanType)dl_MeasurementsFDD = TRUE
. . . . . . . . . . . . . (BooleanType)ul_MeasurementsFDD = TRUE
. . . . . . . . . . . CompressedModeMeasCapabGSMList
. . . . . . . . . . . . CompressedModeMeasCapabGSM
. . . . . . . . . . . . . (RadioFrequencyBandGSM)radioFrequencyBandGSM[4] = 2
. . . . . . . . . . . . . (BooleanType)dl_MeasurementsGSM = FALSE
. . . . . . . . . . . . . (BooleanType)ul_MeasurementsGSM = FALSE
. . . . . . . . . . . . CompressedModeMeasCapabGSM
. . . . . . . . . . . . . (RadioFrequencyBandGSM)radioFrequencyBandGSM[4] = 6
. . . . . . . . . . . . . (BooleanType)dl_MeasurementsGSM = FALSE
. . . . . . . . . . . . . (BooleanType)ul_MeasurementsGSM = TRUE
. . . . . . . . . . . CompressedModeMeasCapabMC
. . . . . . v380NonCriticalExtensions
- Constraint:
car_RRC_ConnSetupCmpl
- BinaryMessage:
30 2a 02 01 ff 02 01 02 0a 05 01 00 00 00 00 4a 8b ff ff e0 00 04 91 a0 51 06 a4 c2 68 46 09 30 20 80 00 80 01 08 89 62 13 89 0c 80

- No.: 1259
- Timestamp: 17:11:29:815_1
- RFN: 5754
- Chip: 5888
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1281
- Timestamp: 17:11:29:942_1
- RFN: 5766
- Chip: 30208
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_GMM_DetachOnSwitchOff:lt_Detach_NMO_I LINE 1
- Message Structure:
RRC_DataInd
. (IntegerType)cellId[0] = -1
. (SS_RB_Identity)rB_Id[0] = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain[0] = 1
. (START_Value)start[20] = '00000000000000000010'B
. DETACHREQUESTMO
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)gMMProtocolDiscriminator[4] = '1000'B
. . (MsgType)msgType[8] = '00000101'B
. . (B4)spare4[4] = '0000'B
. . DetachType
. . . (B1)powOff[1] = '1'B
. . . (B3)type[3] = '011'B
. . GMM_MS_IdentityPTMSI
. . . (IEI8)iei[8] = '00011000'B
. . . (Length)iel[1] = '05'O
. . . (B4)iDigit1[4] = '1111'B
. . . (B1)oddEvenInd[1] = '0'B
. . . (B3)typeOfId[3] = '100'B
. . . (OctetStringType)otherDigits[4] = '12345678'O
. . PTMSI_Signature_tlv
. . . (IEI8)iei[8] = '00011001'B
. . . (Length)iel[1] = '03'O
. . . (OctetStringType)value[3] = 'AB1234'O
- Constraint:
car_PS_InitDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 03 04 04 00 00 20 08 05 0b 18 05 f4 12 34 56 78 19 03 ab 12 34

- No.: 1282
- Timestamp: 17:11:29:943_0
- RFN: 5766
- Chip: 31744
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_GMM_DetachOnSwitchOff:lt_Detach_NMO_I LINE 1
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1291
- Timestamp: 17:11:29:944_2
- RFN: 5766
- Chip: 36096
- Event: Start Timer
- Source: ts_RRC_Delay LINE 1
- Message Structure:
no details available
- Constraint:
t_Dly (1000 Ms)
- BinaryMessage:

- No.: 1296
- Timestamp: 17:11:30:041_1
- RFN: 5776
- Chip: 27648
- Event: Receive
- PCO: CPHY
- Message: CPHY_Out_of_Sync_IND
- Source: RRC_Def1 LINE 19
- Message Structure:
CPHY_Out_of_Sync_IND
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 20
- Constraint:
ca_OutOfSyncInd
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 1298
- Timestamp: 17:11:30:042_0
- RFN: 5776
- Chip: 29184
- Event: Default
- Source: RRC_Def1 LINE 0
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1299
- Timestamp: 17:11:30:042_1
- RFN: 5776
- Chip: 29440
- Event: Default
- Source: ts_RRC_Delay LINE 2
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1304
- Timestamp: 17:11:30:945_0
- RFN: 5867
- Chip: 2304
- Event: Timeout
- Source: ts_RRC_Delay LINE 2
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 1309
- Timestamp: 17:11:30:946_0
- RFN: 5867
- Chip: 7936
- Event: Send
- PCO: UM
- Message: RLC_UM_DATA_REQ
- Source: ts_RRC_ConnRel_AfterSwitchOff:lt_Send_RRC_ConnectionRelease LINE 3
- Message Structure:
RLC_UM_DATA_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 1
. uM_message
. . DL_DCCH_Message
. . . IntegrityCheckInfo
. . . DL_DCCH_MessageType
. . . . RRCConnectionRelease
. . . . . r3
. . . . . . RRCConnectionRelease_r3_IEs
. . . . . . . (IntegerType)rrc_TransactionIdentifier[-1] = 0
. . . . . . . (IntegerType)n_308[-1] = 1
. . . . . . . (ReleaseCause)releaseCause[0] = 0
. . . . . . . Rplmn_Information
. . . . . . laterNonCriticalExtensions
. (BooleanType)specialLI = FALSE
- Constraint:
cas_RRC_ConnRelDCCH
- BinaryMessage:
30 0c 02 01 ff 02 01 01 3c 80 00 01 01 00

- No.: 1311
- Timestamp: 17:11:30:947_1
- RFN: 5867
- Chip: 10240
- Event: Start Timer
- Source: ts_RRC_ConnRel_AfterSwitchOff:lt_Send_RRC_ConnectionRelease LINE 4
- Message Structure:
no details available
- Constraint:
t_Dly (1000 Ms)
- BinaryMessage:

- No.: 1315
- Timestamp: 17:11:31:937_0
- RFN: 5966
- Chip: 13056
- Event: Timeout
- Source: ts_RRC_ConnRel_AfterSwitchOff:lt_Send_RRC_ConnectionRelease LINE 5
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 1316
- Timestamp: 17:11:31:937_1
- RFN: 5966
- Chip: 13312
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ConnRel_AfterSwitchOff:lt_Send_RRC_ConnectionRelease LINE 5
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1322
- Timestamp: 17:11:31:939_0
- RFN: 5966
- Chip: 19200
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 1
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 01 0a 01 00 05 00

- No.: 1326
- Timestamp: 17:11:31:941_0
- RFN: 5966
- Chip: 28160
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 1329
- Timestamp: 17:11:31:942_1
- RFN: 5966
- Chip: 31744
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 2
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 02 0a 01 00 05 00

- No.: 1333
- Timestamp: 17:11:31:949_0
- RFN: 5967
- Chip: 21248
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 1336
- Timestamp: 17:11:31:950_2
- RFN: 5967
- Chip: 24576
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 3
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 03 0a 01 00 05 00

- No.: 1340
- Timestamp: 17:11:31:954_0
- RFN: 5968
- Chip: 1024
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 3
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 1343
- Timestamp: 17:11:31:955_0
- RFN: 5968
- Chip: 4864
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 4
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 04 0a 01 00 05 00

- No.: 1347
- Timestamp: 17:11:31:960_0
- RFN: 5968
- Chip: 25600
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 4
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 1350
- Timestamp: 17:11:31:962_0
- RFN: 5968
- Chip: 31232
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 1
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 136
. . . . . UL_RLC_Mode
. . . . . . UL_UM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (NoExplicitDiscard)timerBasedNoExplicit[0] = 9
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 1
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 1
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_UM_Info
- BinaryMessage:
30 22 02 01 ff 02 01 01 0a 01 00 30 17 30 0d 05 00 30 09 02 02 00 88 30 03 0a 01 09 30 06 02 01 01 02 01 01

- No.: 1354
- Timestamp: 17:11:31:969_0
- RFN: 5969
- Chip: 22016
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 1355
- Timestamp: 17:11:31:971_0
- RFN: 5969
- Chip: 28672
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 3
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 2
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 2
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 2
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 02 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 13 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 02 02 01 02

- No.: 1359
- Timestamp: 17:11:31:984_0
- RFN: 5971
- Chip: 2304
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 4
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 1360
- Timestamp: 17:11:31:986_0
- RFN: 5971
- Chip: 8704
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 5
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 3
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 3
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 3
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 03 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 13 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 03 02 01 03

- No.: 1364
- Timestamp: 17:11:32:000_0
- RFN: 5972
- Chip: 23040
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 6
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 3
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 1365
- Timestamp: 17:11:32:001_0
- RFN: 5972
- Chip: 29184
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 7
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 4
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 4
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 4
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 04 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 13 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 04 02 01 04

- No.: 1369
- Timestamp: 17:11:32:018_0
- RFN: 5974
- Chip: 18176
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 8
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 4
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 1393
- Timestamp: 17:11:32:021_5
- RFN: 5974
- Chip: 29184
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: tc_12_4_1_4c2:lt_TestBody LINE 1
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1399
- Timestamp: 17:11:32:022_4
- RFN: 5974
- Chip: 33792
- Event: Send
- PCO: Ut
- Message: MMI_CmdReq
- Source: ts_MMI_UE_SwitchOn LINE 2
- Message Structure:
MMI_CmdReq
. (IA5StringType)cmd[-1] = "Please switch on the UE"
- Constraint:
ca_MMI_CmdReq
- BinaryMessage:
50 6c 65 61 73 65 20 73 77 69 74 63 68 20 6f 6e 20 74 68 65 20 55 45

- No.: 1403
- Timestamp: 17:11:39:558_0
- RFN: 6728
- Chip: 18432
- Event: Receive
- PCO: Ut
- Message: MMI_CmdCnf
- Source: ts_MMI_UE_SwitchOn LINE 3
- Message Structure:
MMI_CmdCnf
. (BooleanType)result = TRUE
. (IA5StringType)resultString[0] = ""
- Constraint:
ca_MMI_CmdCnf
- BinaryMessage:
80

- No.: 1424
- Timestamp: 17:11:48:348_0
- RFN: 7607
- Chip: 22528
- Event: Receive
- PCO: TM
- Message: RLC_TR_DATA_IND
- Source: ts_RRC_ConnEst:lt_RcvConnReq LINE 2
- Message Structure:
RLC_TR_DATA_IND
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 0
. tM_message
. . UL_CCCH_Message
. . . IntegrityCheckInfo
. . . UL_CCCH_MessageType
. . . . RRCConnectionRequest
. . . . . InitialUE_Identity
. . . . . . TMSI_and_LAI_GSM_MAP
. . . . . . . (BitStringType)tmsi[32] = "00010010001101000101011001111000"
. . . . . . . LAI
. . . . . . . . PLMN_Identity
. . . . . . . . . MCC
. . . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . . (IntegerType)_elem[4] = 1
. . . . . . . . . MNC
. . . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . . (IntegerType)_elem[4] = 1
. . . . . . . . (BitStringType)lac[16] = '0000000000000001'B
. . . . . (EstablishmentCause)establishmentCause[5] = 12
. . . . . (ProtocolErrorIndicator)protocolErrorIndicator[1] = 0
. . . . . MeasuredResultsOnRACH
. . . . . v3d0NonCriticalExtensions
- Constraint:
car_RRC_ConnReq
- BinaryMessage:
30 11 02 01 00 02 01 00 21 12 34 56 78 00 10 08 00 0b 00

- No.: 1428
- Timestamp: 17:11:48:358_0
- RFN: 7608
- Chip: 22016
- Event: Send
- PCO: UM
- Message: RLC_UM_DATA_REQ
- Source: ts_RRC_ConnEst:lt_Send_ConnSetUp LINE 22
- Message Structure:
RLC_UM_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 0
. uM_message
. . DL_CCCH_Message
. . . IntegrityCheckInfo
. . . DL_CCCH_MessageType
. . . . RRCConnectionSetup
. . . . . r3
. . . . . . RRCConnectionSetup_r3_IEs
. . . . . . . InitialUE_Identity
. . . . . . . . TMSI_and_LAI_GSM_MAP
. . . . . . . . . (BitStringType)tmsi[32] = "00010010001101000101011001111000"
. . . . . . . . . LAI
. . . . . . . . . . PLMN_Identity
. . . . . . . . . . . MCC
. . . . . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . . . . (IntegerType)_elem[4] = 1
. . . . . . . . . . . MNC
. . . . . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . . . . (IntegerType)_elem[4] = 1
. . . . . . . . . . (BitStringType)lac[16] = '0000000000000001'B
. . . . . . . (IntegerType)rrc_TransactionIdentifier[-1] = 0
. . . . . . . (IntegerType)activationTime[-1] = -
. . . . . . . U_RNTI
. . . . . . . . (BitStringType)srnc_Identity[12] = "000000000001"
. . . . . . . . (BitStringType)s_RNTI[20] = "00000000000000000001"
. . . . . . . (BitStringType)new_c_RNTI[16] = -
. . . . . . . (RRC_StateIndicator)rrc_StateIndicator[0] = 0
. . . . . . . (IntegerType)utran_DRX_CycleLengthCoeff[-1] = 9
. . . . . . . CapabilityUpdateRequirement
. . . . . . . . (BooleanType)ue_RadioCapabilityFDDUpdateRequirement = TRUE
. . . . . . . . (BooleanType)ue_RadioCapabilityTDDUpdateRequirement = FALSE
. . . . . . . . SystemSpecificCapUpdateReqList
. . . . . . . . . (SystemSpecificCapUpdateReq)_elem[0] = 0
. . . . . . . SRB_InformationSetupList2
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity[-1] = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_UM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 1
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex[-1] = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 1
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity[-1] = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 2
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 2
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 2
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 2
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex[-1] = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 2
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 2
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity[-1] = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 3
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 3
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 3
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 3
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex[-1] = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 3
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 3
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity[-1] = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 4
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 4
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 4
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 4
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex[-1] = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 4
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 4
. . . . . . . UL_CommonTransChInfo
. . . . . . . . TFC_Subset
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . TFCS
. . . . . . . . . . . ExplicitTFCS_Configuration
. . . . . . . . . . . . TFCS_ReconfAdd
. . . . . . . . . . . . . ctfcSize
. . . . . . . . . . . . . . ctfc2Bit
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . . . . . . . (IntegerType)ctfc2[-1] = 0
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . . . . . . . (IntegerType)ctfc2[-1] = 1
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC[-1] = 11
. . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaD[-1] = 15
. . . . . . . . . . . . . . . . . . . (IntegerType)referenceTFC_ID[-1] = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . UL_AddReconfTransChInfoList
. . . . . . . . UL_AddReconfTransChInformation
. . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType[0] = 0
. . . . . . . . . (IntegerType)transportChannelIdentity[-1] = 5
. . . . . . . . . TransportFormatSet
. . . . . . . . . . DedicatedTransChTFS
. . . . . . . . . . . tti
. . . . . . . . . . . . DedicatedDynamicTF_InfoList
. . . . . . . . . . . . . DedicatedDynamicTF_Info
. . . . . . . . . . . . . . rlc_Size
. . . . . . . . . . . . . . . BitModeRLC_SizeInfo
. . . . . . . . . . . . . . . . sizeType2
. . . . . . . . . . . . . . . . . (IntegerType)part1[-1] = 2
. . . . . . . . . . . . . . . . . (IntegerType)part2[-1] = -
. . . . . . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . LogicalChannelList
. . . . . . . . . . . SemistaticTF_Information
. . . . . . . . . . . . ChannelCodingType
. . . . . . . . . . . . . (CodingRate)convolutional[0] = 1
. . . . . . . . . . . . (IntegerType)rateMatchingAttribute[-1] = 192
. . . . . . . . . . . . (CRC_Size)crc_Size[0] = 3
. . . . . . . DL_CommonTransChInfo
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . dl_Parameters
. . . . . . . DL_AddReconfTransChInfoList
. . . . . . . . DL_AddReconfTransChInformation
. . . . . . . . . (DL_TrCH_Type)dl_TransportChannelType[0] = 0
. . . . . . . . . (IntegerType)dl_transportChannelIdentity[-1] = 10
. . . . . . . . . tfs_SignallingMode
. . . . . . . . . . UL_TransportChannelIdentity
. . . . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType[0] = 0
. . . . . . . . . . . (IntegerType)ul_TransportChannelIdentity[-1] = 5
. . . . . . . . . QualityTarget
. . . . . . . . . . (IntegerType)bler_QualityValue[-1] = -20
. . . . . . . . . TM_SignallingInfo
. . . . . . . FrequencyInfo
. . . . . . . (IntegerType)maxAllowedUL_TX_Power[-1] = -
. . . . . . . UL_ChannelRequirement
. . . . . . . . UL_DPCH_Info
. . . . . . . . . UL_DPCH_PowerControlInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (IntegerType)dpcch_PowerOffset[-1] = -40
. . . . . . . . . . . (IntegerType)pc_Preamble[-1] = 1
. . . . . . . . . . . (IntegerType)sRB_delay[-1] = 7
. . . . . . . . . . . PowerControlAlgorithm
. . . . . . . . . . . . (IntegerType)algorithm1[-1] = 1
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (ScramblingCodeType)scramblingCodeType[0] = 1
. . . . . . . . . . . (IntegerType)scramblingCode[-1] = 0
. . . . . . . . . . . (IntegerType)numberOfDPDCH[-1] = -
. . . . . . . . . . . (SpreadingFactor)spreadingFactor[0] = 4
. . . . . . . . . . . (BooleanType)tfci_Existence = TRUE
. . . . . . . . . . . (IntegerType)numberOfFBI_Bits[-1] = -
. . . . . . . . . . . (PuncturingLimit)puncturingLimit[0] = 15
. . . . . . . DL_CommonInformation
. . . . . . . . DL_DPCH_InfoCommon
. . . . . . . . . cfnHandling
. . . . . . . . . . initialise
. . . . . . . . . . . (IntegerType)cfntargetsfnframeoffset[-1] = -
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . DL_DPCH_PowerControlInfo
. . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . (DPC_Mode)dpc_Mode[0] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPilot_pdpdch[-1] = 0
. . . . . . . . . . . Dl_rate_matching_restriction
. . . . . . . . . . . SF512_AndPilot
. . . . . . . . . . . . (PilotBits128)sfd128[0] = 0
. . . . . . . . . . . (PositionFixedOrFlexible)positionFixedOrFlexible[0] = 0
. . . . . . . . . . . (BooleanType)tfci_Existence = FALSE
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . (IntegerType)defaultDPCH_OffsetValue[-1] = 459
. . . . . . . . . . DPCH_CompressedModeInfo
. . . . . . . . . . (TX_DiversityMode)tx_DiversityMode[0] = 0
. . . . . . . . . . SSDT_Information
. . . . . . . DL_InformationPerRL_List
. . . . . . . . DL_InformationPerRL
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . PrimaryCPICH_Info
. . . . . . . . . . . . (IntegerType)primaryScramblingCode[-1] = 100
. . . . . . . . . . . PDSCH_SHO_DCH_Info
. . . . . . . . . . . PDSCH_CodeMapping
. . . . . . . . . DL_DPCH_InfoPerRL
. . . . . . . . . . fdd
. . . . . . . . . . . (PCPICH_UsageForChannelEst)pCPICH_UsageForChannelEst[0] = 0
. . . . . . . . . . . (IntegerType)dpch_FrameOffset[-1] = 18
. . . . . . . . . . . SecondaryCPICH_Info
. . . . . . . . . . . DL_ChannelisationCodeList
. . . . . . . . . . . . DL_ChannelisationCode
. . . . . . . . . . . . . (IntegerType)secondaryScramblingCode[-1] = 1
. . . . . . . . . . . . . SF512_AndCodeNumber
. . . . . . . . . . . . . . (IntegerType)sf128[-1] = 0
. . . . . . . . . . . . . (ScramblingCodeChange)scramblingCodeChange[0] = 1
. . . . . . . . . . . (IntegerType)tpc_CombinationIndex[-1] = 0
. . . . . . . . . . . (SSDT_CellIdentity)ssdt_CellIdentity[0] = -
. . . . . . . . . . . (ClosedLoopTimingAdjMode)closedLoopTimingAdjMode[0] = -
. . . . . . . . . SCCPCH_InfoForFACH
. . . . . . laterNonCriticalExtensions
. (BooleanType)specialLI = TRUE
- Constraint:
cas_RRC_ConnSetup
- BinaryMessage:
30 78 02 01 00 02 01 00 30 e7 22 46 8a cf 00 02 01 00 01 00 04 00 00 4d 82 69 3a 10 10 89 0d 42 00 02 81 9e 8e 46 c9 a6 7c 9c 4e 74 20 a5 12 3a 8c 00 15 13 3d 1c 8d 93 4c f9 38 9c e8 42 52 24 b5 28 00 4a 46 7a 39 1b 26 99 f2 71 39 d0 86 b4 49 ea 70 00 d4 c8 00 06 25 2b f0 02 00 08 82 23 bf 66 08 98 95 a5 47 a2 00 00 01 3f 90 0a 14 e5 82 06 40 09 0c 28 08 01 01 ff

- No.: 1449
- Timestamp: 17:11:48:380_4
- RFN: 7610
- Chip: 31744
- Event: Start Timer
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 3
- Message Structure:
no details available
- Constraint:
t_WaitMS (13500 Ms)
- BinaryMessage:

- No.: 1456
- Timestamp: 17:11:48:590_0
- RFN: 7631
- Chip: 29184
- Event: Receive
- PCO: CPHY
- Message: CPHY_Sync_IND
- Source: RRC_DefConnEst LINE 5
- Message Structure:
CPHY_Sync_IND
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 20
- Constraint:
ca_SyncInd
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 1458
- Timestamp: 17:11:48:590_2
- RFN: 7631
- Chip: 30464
- Event: Default
- Source: RRC_DefConnEst LINE 0
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1459
- Timestamp: 17:11:48:590_3
- RFN: 7631
- Chip: 30976
- Event: Default
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1466
- Timestamp: 17:11:48:712_0
- RFN: 7643
- Chip: 36864
- Event: Receive
- PCO: AM
- Message: RLC_AM_DATA_IND
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
RLC_AM_DATA_IND
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 2
. IntegrityResult
. . (IntegrityStatus)integrityUsed[0] = 4294967296
. aM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . UL_DCCH_MessageType
. . . . RRCConnectionSetupComplete
. . . . . (IntegerType)rrc_TransactionIdentifier[2] = 0
. . . . . STARTList
. . . . . . STARTSingle
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity[1] = 0
. . . . . . . (BitStringType)start_Value[20] = "11111111111111111111"
. . . . . . STARTSingle
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity[1] = 1
. . . . . . . (BitStringType)start_Value[20] = "00000000000000000010"
. . . . . UE_RadioAccessCapability
. . . . . . (AccessStratumReleaseIndicator)accessStratumReleaseIndicator[0] = 0
. . . . . . PDCP_Capability
. . . . . . . (BooleanType)losslessSRNS_RelocationSupport = TRUE
. . . . . . . supportForRfc2507
. . . . . . RLC_Capability
. . . . . . . (TotalRLC_AM_BufferSize)totalRLC_AM_BufferSize[3] = 2
. . . . . . . (MaximumRLC_WindowSize)maximumRLC_WindowSize[1] = 0
. . . . . . . (MaximumAM_EntityNumberRLC_Cap)maximumAM_EntityNumber[3] = 3
. . . . . . TransportChannelCapability
. . . . . . . DL_TransChCapability
. . . . . . . . (MaxNoBits)maxNoBitsReceived[4] = 4
. . . . . . . . (MaxNoBits)maxConvCodeBitsReceived[4] = 0
. . . . . . . . TurboSupport
. . . . . . . . . (MaxNoBits)supported[4] = 4
. . . . . . . . (MaxSimultaneousTransChsDL)maxSimultaneousTransChs[2] = 1
. . . . . . . . (IntegerType)maxSimultaneousCCTrCH_Count[3] = 1
. . . . . . . . (MaxTransportBlocksDL)maxReceivedTransportBlocks[4] = 3
. . . . . . . . (MaxNumberOfTFC_DL)maxNumberOfTFC[4] = 5
. . . . . . . . (MaxNumberOfTF)maxNumberOfTF[3] = 1
. . . . . . . UL_TransChCapability
. . . . . . . . (MaxNoBits)maxNoBitsTransmitted[4] = 3
. . . . . . . . (MaxNoBits)maxConvCodeBitsTransmitted[4] = 0
. . . . . . . . TurboSupport
. . . . . . . . . (MaxNoBits)supported[4] = 3
. . . . . . . . (MaxSimultaneousTransChsUL)maxSimultaneousTransChs[3] = 2
. . . . . . . . modeSpecificInfo
. . . . . . . . (MaxTransportBlocksUL)maxTransmittedBlocks[4] = 2
. . . . . . . . (MaxNumberOfTFC_UL)maxNumberOfTFC[4] = 3
. . . . . . . . (MaxNumberOfTF)maxNumberOfTF[3] = 0
. . . . . . RF_Capability
. . . . . . . fddRF_Capability
. . . . . . . tddRF_Capability
. . . . . . PhysicalChannelCapability
. . . . . . . fddPhysChCapability
. . . . . . . . DL_PhysChCapabilityFDD
. . . . . . . . . (IntegerType)maxNoDPCH_PDSCH_Codes[3] = 3
. . . . . . . . . (MaxNoPhysChBitsReceived)maxNoPhysChBitsReceived[4] = 6
. . . . . . . . . (BooleanType)supportForSF_512 = FALSE
. . . . . . . . . (BooleanType)supportOfPDSCH = FALSE
. . . . . . . . . SimultaneousSCCPCH_DPCH_Reception
. . . . . . . . UL_PhysChCapabilityFDD
. . . . . . . . . (MaxNoDPDCH_BitsTransmitted)maxNoDPDCH_BitsTransmitted[4] = 2
. . . . . . . . . (BooleanType)supportOfPCPCH = FALSE
. . . . . . . tddPhysChCapability
. . . . . . UE_MultiModeRAT_Capability
. . . . . . . MultiRAT_Capability
. . . . . . . . (BooleanType)supportOfGSM = FALSE
. . . . . . . . (BooleanType)supportOfMulticarrier = FALSE
. . . . . . . (MultiModeCapability)multiModeCapability[2] = 1
. . . . . . SecurityCapability
. . . . . . . (BitStringType)cipheringAlgorithmCap[16] = '0000000000000001'B
. . . . . . . (BitStringType)integrityProtectionAlgorithmCap[16] = '0000000000000010'B
. . . . . . UE_Positioning_Capability
. . . . . . . (BooleanType)standaloneLocMethodsSupported = FALSE
. . . . . . . (BooleanType)ue_BasedOTDOA_Supported = FALSE
. . . . . . . (NetworkAssistedGPS_Supported)networkAssistedGPS_Supported[2] = 1
. . . . . . . (BooleanType)supportForUE_GPS_TimingOfCellFrames = FALSE
. . . . . . . (BooleanType)supportForIPDL = FALSE
. . . . . . MeasurementCapability
. . . . . v370NonCriticalExtensions
. . . . . . RRCConnectionSetupComplete_v370ext
. . . . . . . UE_RadioAccessCapability_v370ext
. . . . . . . . UE_RadioAccessCapabBandFDDList
. . . . . . . . . UE_RadioAccessCapabBandFDD
. . . . . . . . . . (RadioFrequencyBandFDD)radioFrequencyBandFDD[3] = 1
. . . . . . . . . . fddRF_Capability
. . . . . . . . . . . (UE_PowerClassExt)ue_PowerClass[3] = 3
. . . . . . . . . . . (TxRxFrequencySeparation)txRxFrequencySeparation[2] = 0
. . . . . . . . . . MeasurementCapabilityExt
. . . . . . . . . . . CompressedModeMeasCapabFDDList
. . . . . . . . . . . . CompressedModeMeasCapabFDD
. . . . . . . . . . . . . (RadioFrequencyBandFDD)radioFrequencyBandFDD[3] = 1
. . . . . . . . . . . . . (BooleanType)dl_MeasurementsFDD = TRUE
. . . . . . . . . . . . . (BooleanType)ul_MeasurementsFDD = TRUE
. . . . . . . . . . . CompressedModeMeasCapabGSMList
. . . . . . . . . . . . CompressedModeMeasCapabGSM
. . . . . . . . . . . . . (RadioFrequencyBandGSM)radioFrequencyBandGSM[4] = 2
. . . . . . . . . . . . . (BooleanType)dl_MeasurementsGSM = FALSE
. . . . . . . . . . . . . (BooleanType)ul_MeasurementsGSM = FALSE
. . . . . . . . . . . . CompressedModeMeasCapabGSM
. . . . . . . . . . . . . (RadioFrequencyBandGSM)radioFrequencyBandGSM[4] = 6
. . . . . . . . . . . . . (BooleanType)dl_MeasurementsGSM = FALSE
. . . . . . . . . . . . . (BooleanType)ul_MeasurementsGSM = TRUE
. . . . . . . . . . . CompressedModeMeasCapabMC
. . . . . . v380NonCriticalExtensions
- Constraint:
car_RRC_ConnSetupCmpl
- BinaryMessage:
30 2a 02 01 ff 02 01 02 0a 05 01 00 00 00 00 4a 8b ff ff e0 00 04 91 a0 51 06 a4 c2 68 46 09 30 20 80 00 80 01 08 89 62 13 89 0c 80

- No.: 1468
- Timestamp: 17:11:48:714_1
- RFN: 7644
- Chip: 6656
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1491
- Timestamp: 17:11:48:851_0
- RFN: 7657
- Chip: 32512
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: tc_12_4_1_4c2:lt_Attach_Steps_3To4 LINE 1
- Message Structure:
RRC_DataInd
. (IntegerType)cellId[0] = -1
. (SS_RB_Identity)rB_Id[0] = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain[0] = 1
. (START_Value)start[20] = '00000000000000000010'B
. ATTACHREQUEST
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)gMMProtocolDiscriminator[4] = '1000'B
. . (MsgType)msgType[8] = '00000001'B
. . MS_NetworkCap_lv
. . . (Length)iel[1] = '02'O
. . . (OctetStringType)value[2] = 'C500'O
. . CiphKeySeqNum
. . . (B1)spare1[1] = '0'B
. . . (KeySeq)keySeq[3] = '000'B
. . AttachType
. . . (B1)pre_for[1] = '0'B
. . . (B3)type[3] = '011'B
. . DRXparamter
. . . (B8)splitPGcycleCode[8] = '00001101'B
. . . (B4)cnDRXcoef[4] = '0000'B
. . . (B1)splitOnCCCH[1] = '0'B
. . . (B3)nonDRXtimer[3] = '011'B
. . MS_Identity_lv
. . . (Length)iel[1] = '05'O
. . . (B4)iDigit1[4] = '1111'B
. . . (B1)oddEvenInd[1] = '0'B
. . . (B3)typeOfId[3] = '100'B
. . . (OctetStringType)otherDigits[4] = '12345678'O
. . RAI_v
. . . (OctetStringType)plmn[3] = '00F110'O
. . . (OctetStringType)lac[2] = '0001'O
. . . (OctetStringType)rac[1] = '05'O
. . MSRadioAccessCap_lv
. . . (Length)iel[1] = '05'O
. . . (OctetStringType)value[5] = '02C2000600'O
. . PTMSI_Signature
. . GPRS_Timer
. . TMSI_Status
- Constraint:
car_PS_InitDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 03 04 04 00 00 20 08 01 02 c5 00 03 0d 03 05 f4 12 34 56 78 00 f1 10 00 01 05 05 02 c2 00 06 00

- No.: 1528
- Timestamp: 17:11:48:857_0
- RFN: 7658
- Chip: 18176
- Event: Send
- PCO: Dc
- Message: RRC_DataReq
- Source: ts_GMM_Authentication LINE 2
- Message Structure:
RRC_DataReq
. (IntegerType)cellId[-1] = -1
. (SS_RB_Identity)rB_Id[-1] = 3
. (LogicChGERAN)ch[-1] = -
. (SapId)sapId[1] = -
. (SS_CN_DomainIdentity)cN_Domain[-1] = 1
. AUTHENTICATIONANDCIPHERINGREQUEST
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)gMMProtocolDiscriminator[4] = '1000'B
. . (MsgType)msgType[8] = '00010010'B
. . IMEISVRequest
. . . (B1)spare1[1] = '0'B
. . . (B3)value[3] = '000'B
. . CiphAlgorithm
. . . (B1)spare1[1] = '0'B
. . . (B3)algorithm[3] = '001'B
. . AC_ReferenceNumber
. . . (B4)value[4] = '0011'B
. . ForceToStandby
. . . (B1)spare[1] = '0'B
. . . (B3)value[3] = '000'B
. . AuthenticationParamterRAND
. . . (IEI8)iei[8] = '00100001'B
. . . (BitStringType)randValue[128] = '01010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101'B
. . CiphKeySeqNum_tv
. . . (IEI4)iei[4] = '1000'B
. . . (B1)spare1[1] = '0'B
. . . (KeySeq)keySeq[3] = '001'B
. . GMM_AUTN
. . . (IEI8)iei[8] = '00101000'B
. . . (Length)iel[1] = '10'O
. . . (BitStringType)aUTN[128] = '01100110000100010000000000110011001000101101110100000000000000000101010101000100011101110110011000010001000000000011001100100010'B
- Constraint:
ca_PS_DataReq
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 08 12 01 30 21 55 55 55 55 55 55 55 55 55 55 55 55 55 55 55 55 81 28 10 66 11 00 33 22 dd 00 00 55 44 77 66 11 00 33 22

- No.: 1532
- Timestamp: 17:11:49:230_0
- RFN: 7695
- Chip: 30464
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_GMM_Authentication LINE 3
- Message Structure:
RRC_DataInd
. (IntegerType)cellId[0] = -1
. (SS_RB_Identity)rB_Id[0] = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain[0] = 1
. (START_Value)start[0] = -
. AUTHENTICATIONANDCIPHERINGRESPONSE
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)gMMProtocolDiscriminator[4] = '1000'B
. . (MsgType)msgType[8] = '00010011'B
. . (B4)spare4[4] = '0000'B
. . AC_ReferenceNumber
. . . (B4)value[4] = '0011'B
. . AuthRsp_tv
. . . (IEI8)iei[8] = '00100010'B
. . . (BitStringType)value[32] = '01010101010001000111011101100110'B
. . GMM_MS_Identity
. . AuthRspExt
. . . (IEI8)iei[8] = '00101001'B
. . . (Length)iel[1] = '04'O
. . . (BitStringType)rES[32] = '00010001000000000011001100100010'B
- Constraint:
car_PS_UplinkDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 08 13 03 22 55 44 77 66 29 04 11 00 33 22

- No.: 1535
- Timestamp: 17:11:49:231_1
- RFN: 7695
- Chip: 33280
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_GMM_Authentication LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1596
- Timestamp: 17:11:49:238_4
- RFN: 7696
- Chip: 24576
- Event: Send
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_REQ
- Source: ts_SS_DownloadSecurityKey:lt_DownloadKeyCRLC LINE 1
- Message Structure:
CRLC_SecurityMode_Config_REQ
. (IntegerType)cellId[-1] = -1
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity[0] = 1
. . (BitStringType)startValue[20] = "00000000000000000000"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = '01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100'B
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CRLC_SecurityModeCfgReq
- BinaryMessage:
30 21 02 01 ff 30 1c 0a 01 01 03 04 04 00 00 00 03 11 00 77 66 11 00 33 22 dd cc ff ee 99 88 bb aa 55 44

- No.: 1597
- Timestamp: 17:11:49:239_0
- RFN: 7696
- Chip: 26368
- Event: Receive
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_CNF
- Source: ts_SS_DownloadSecurityKey:lt_DownloadKeyCRLC LINE 2
- Message Structure:
CRLC_SecurityMode_Config_CNF
. (IntegerType)cellId[0] = -1
- Constraint:
ca_CRLC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1604
- Timestamp: 17:11:49:240_2
- RFN: 7696
- Chip: 31232
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 1
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 0
. (IntegerType)count_I_LSB_UL[-1] = -
. (IntegerType)count_I_LSB_DL[-1] = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 00 02 01 00 02 01 00

- No.: 1605
- Timestamp: 17:11:49:241_0
- RFN: 7696
- Chip: 33024
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 2
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 0
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 00 02 01 00

- No.: 1606
- Timestamp: 17:11:49:241_1
- RFN: 7696
- Chip: 34560
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 3
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 1
. (IntegerType)count_I_LSB_UL[-1] = -
. (IntegerType)count_I_LSB_DL[-1] = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 01 02 01 00

- No.: 1607
- Timestamp: 17:11:49:241_2
- RFN: 7696
- Chip: 36352
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 4
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 1
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 1608
- Timestamp: 17:11:49:242_0
- RFN: 7696
- Chip: 38144
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 5
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 2
. (IntegerType)count_I_LSB_UL[-1] = -
. (IntegerType)count_I_LSB_DL[-1] = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 02 02 01 00

- No.: 1609
- Timestamp: 17:11:49:242_1
- RFN: 7697
- Chip: 1280
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 6
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 2
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 1610
- Timestamp: 17:11:49:243_0
- RFN: 7697
- Chip: 3072
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 7
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 3
. (IntegerType)count_I_LSB_UL[-1] = -
. (IntegerType)count_I_LSB_DL[-1] = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 03 02 01 00

- No.: 1611
- Timestamp: 17:11:49:243_1
- RFN: 7697
- Chip: 4608
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 8
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 3
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 1612
- Timestamp: 17:11:49:244_0
- RFN: 7697
- Chip: 6656
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 9
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 4
. (IntegerType)count_I_LSB_UL[-1] = -
. (IntegerType)count_I_LSB_DL[-1] = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 04 02 01 00

- No.: 1613
- Timestamp: 17:11:49:244_1
- RFN: 7697
- Chip: 8448
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 10
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 4
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 1617
- Timestamp: 17:11:49:245_1
- RFN: 7697
- Chip: 12032
- Event: Send
- PCO: CRLC
- Message: CRLC_Integrity_Activate_REQ
- Source: ts_CRLC_DL_Integrity LINE 1
- Message Structure:
CRLC_Integrity_Activate_REQ
. (IntegerType)cellId[-1] = -1
. (CN_DomainIdentity)cn_DomainIdentity[0] = 1
. IntegrityActivationInfo
. . IntegrityProtectionModeInfo
. . . IntegrityProtectionModeCommand
. . . . startIntegrityProtection
. . . . . (BitStringType)integrityProtInitNumber[32] = "00000000000000000000000000000001"
. . . (IntegrityProtectionAlgorithm)integrityProtectionAlgorithm[0] = 0
- Constraint:
ca_CRLC_DL_IntegrityActivateReq
- BinaryMessage:
30 14 02 01 ff 0a 01 01 30 0c 30 07 03 05 00 00 00 00 01 0a 01 00

- No.: 1618
- Timestamp: 17:11:49:246_0
- RFN: 7697
- Chip: 14336
- Event: Receive
- PCO: CRLC
- Message: CRLC_Integrity_Activate_CNF
- Source: ts_CRLC_DL_Integrity LINE 2
- Message Structure:
CRLC_Integrity_Activate_CNF
. (IntegerType)cellId[0] = -1
- Constraint:
ca_CRLC_IntegrityActivateCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1625
- Timestamp: 17:11:49:247_1
- RFN: 7697
- Chip: 19456
- Event: Send
- PCO: CRLC
- Message: CRLC_Integrity_Activate_REQ
- Source: ts_RB2_UL_IntegrityActivate LINE 1
- Message Structure:
CRLC_Integrity_Activate_REQ
. (IntegerType)cellId[-1] = -1
. (CN_DomainIdentity)cn_DomainIdentity[0] = 1
. IntegrityActivationInfo
. . IntegrityProtActivationInfoList
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity[-1] = 2
. . . . (IntegerType)rrc_MessageSequenceNumber[-1] = 0
- Constraint:
ca_CRLC_UL_IntegrityActivateReq
- BinaryMessage:
30 10 02 01 ff 0a 01 01 30 08 30 06 02 01 02 02 01 00

- No.: 1626
- Timestamp: 17:11:49:247_2
- RFN: 7697
- Chip: 20992
- Event: Receive
- PCO: CRLC
- Message: CRLC_Integrity_Activate_CNF
- Source: ts_RB2_UL_IntegrityActivate LINE 2
- Message Structure:
CRLC_Integrity_Activate_CNF
. (IntegerType)cellId[0] = -1
- Constraint:
ca_CRLC_IntegrityActivateCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1633
- Timestamp: 17:11:49:249_0
- RFN: 7697
- Chip: 28928
- Event: Send
- PCO: AM
- Message: RLC_AM_DATA_REQ
- Source: ts_RRC_Security:lt_SendSecurityModeCommand LINE 8
- Message Structure:
RLC_AM_DATA_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 2
. AmConfirmationRequest
. aM_message
. . DL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00000000000000000000000000000000"
. . . . (IntegerType)rrc_MessageSequenceNumber[-1] = 0
. . . DL_DCCH_MessageType
. . . . SecurityModeCommand
. . . . . r3
. . . . . . SecurityModeCommand_r3_IEs
. . . . . . . (IntegerType)rrc_TransactionIdentifier[-1] = 0
. . . . . . . SecurityCapability
. . . . . . . . (BitStringType)cipheringAlgorithmCap[16] = '0000000000000001'B
. . . . . . . . (BitStringType)integrityProtectionAlgorithmCap[16] = '0000000000000010'B
. . . . . . . CipheringModeInfo
. . . . . . . IntegrityProtectionModeInfo
. . . . . . . . IntegrityProtectionModeCommand
. . . . . . . . . startIntegrityProtection
. . . . . . . . . . (BitStringType)integrityProtInitNumber[32] = "00000000000000000000000000000001"
. . . . . . . . (IntegrityProtectionAlgorithm)integrityProtectionAlgorithm[0] = 0
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity[0] = 1
. . . . . . . InterRAT_UE_SecurityCapList
. . . . . . . . InterRAT_UE_SecurityCapability
. . . . . . . . . gsm
. . . . . . . . . . (BitStringType)gsmSecurityCapability[7] = "0000000"
. . . . . . laterNonCriticalExtensions
- Constraint:
cas_RRC_SecModeCmd
- BinaryMessage:
30 18 02 01 ff 02 01 02 05 00 80 00 00 00 04 06 00 00 80 01 40 00 00 00 30 00

- No.: 1642
- Timestamp: 17:11:49:391_0
- RFN: 7711
- Chip: 31488
- Event: Receive
- PCO: AM
- Message: RLC_AM_DATA_IND
- Source: ts_RRC_Security:lt_StartSecurity_UE LINE 8
- Message Structure:
RLC_AM_DATA_IND
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 2
. IntegrityResult
. . (IntegrityStatus)integrityUsed[0] = 0
. aM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "01100100010100101000000110010100"
. . . . (IntegerType)rrc_MessageSequenceNumber[4] = 1
. . . UL_DCCH_MessageType
. . . . SecurityModeComplete
. . . . . (IntegerType)rrc_TransactionIdentifier[2] = 0
. . . . . IntegrityProtActivationInfo
. . . . . . RRC_MessageSequenceNumberList
. . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . (IntegerType)_elem[4] = 0
. . . . . laterNonCriticalExtensions
- Constraint:
car_RRC_SecModeCmpl
- BinaryMessage:
30 12 02 01 ff 02 01 02 0a 01 00 b2 29 40 ca 0d 21 00 00 00

- No.: 1643
- Timestamp: 17:11:49:391_1
- RFN: 7711
- Chip: 33024
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_Security:lt_StartSecurity_UE LINE 8
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1645
- Timestamp: 17:11:49:392_0
- RFN: 7711
- Chip: 36352
- Event: Send
- PCO: CRLC
- Message: CRLC_Integrity_Activate_REQ
- Source: ts_CRLC_UL_Integrity LINE 1
- Message Structure:
CRLC_Integrity_Activate_REQ
. (IntegerType)cellId[-1] = -1
. (CN_DomainIdentity)cn_DomainIdentity[0] = 1
. IntegrityActivationInfo
. . IntegrityProtActivationInfoList
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity[-1] = 0
. . . . (IntegerType)rrc_MessageSequenceNumber[-1] = 0
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity[-1] = 1
. . . . (IntegerType)rrc_MessageSequenceNumber[-1] = 0
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity[-1] = 3
. . . . (IntegerType)rrc_MessageSequenceNumber[-1] = 0
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity[-1] = 4
. . . . (IntegerType)rrc_MessageSequenceNumber[-1] = 0
- Constraint:
ca_CRLC_UL_IntegrityActivateReq
- BinaryMessage:
30 28 02 01 ff 0a 01 01 30 20 30 06 02 01 00 02 01 00 30 06 02 01 01 02 01 00 30 06 02 01 03 02 01 00 30 06 02 01 04 02 01 00

- No.: 1646
- Timestamp: 17:11:49:392_1
- RFN: 7712
- Chip: 0
- Event: Receive
- PCO: CRLC
- Message: CRLC_Integrity_Activate_CNF
- Source: ts_CRLC_UL_Integrity LINE 2
- Message Structure:
CRLC_Integrity_Activate_CNF
. (IntegerType)cellId[0] = -1
- Constraint:
ca_CRLC_IntegrityActivateCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1652
- Timestamp: 17:11:49:394_0
- RFN: 7712
- Chip: 6144
- Event: Send
- PCO: Dc
- Message: RRC_DataReq
- Source: tc_12_4_1_4c2:lt_Attach_Steps_3To4 LINE 4
- Message Structure:
RRC_DataReq
. (IntegerType)cellId[-1] = -1
. (SS_RB_Identity)rB_Id[-1] = 3
. (LogicChGERAN)ch[-1] = -
. (SapId)sapId[1] = -
. (SS_CN_DomainIdentity)cN_Domain[-1] = 1
. ATTACHACCEPT
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)gMMProtocolDiscriminator[4] = '1000'B
. . (MsgType)msgType[8] = '00000010'B
. . ForceToStandby
. . . (B1)spare[1] = '0'B
. . . (B3)value[3] = '000'B
. . AttachResult
. . . (B1)spare[1] = '0'B
. . . (B3)result[3] = '011'B
. . GPRS_Timer_v
. . . (B3)unit[3] = '001'B
. . . (B5)value[5] = '00110'B
. . (B4)spare[4] = '0000'B
. . RadioPriority_v
. . . (B1)spare[1] = '0'B
. . . (B3)value[3] = '100'B
. . RAI_v
. . . (OctetStringType)plmn[3] = '00F110'O
. . . (OctetStringType)lac[2] = '0001'O
. . . (OctetStringType)rac[1] = '05'O
. . PTMSI_Signature
. . . (IEI8)iei[8] = '00011001'B
. . . (OctetStringType)value[3] = 'AB1237'O
. . GPRS_Timer
. . GMM_MS_IdentityPTMSI
. . . (IEI8)iei[8] = '00011000'B
. . . (Length)iel[1] = '05'O
. . . (B4)iDigit1[4] = '1111'B
. . . (B1)oddEvenInd[1] = '0'B
. . . (B3)typeOfId[3] = '100'B
. . . (OctetStringType)otherDigits[-1] = '09876543'O
. . GMM_MS_Identity
. . . (IEI8)iei[8] = '00100011'B
. . . (Length)iel[1] = '08'O
. . . (B4)iDigit1[4] = '0000'B
. . . (B1)oddEvenInd[1] = '1'B
. . . (B3)typeOfId[3] = '001'B
. . . (OctetStringType)otherDigits[-1] = '10101032547698'O
. . GMM_Cause
. . GPRS_Timer
. . CellNotification
. . PLMN_List
- Constraint:
ca_PS_DataReq
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 08 02 03 26 04 00 f1 10 00 01 05 19 ab 12 37 18 05 f4 09 87 65 43 23 08 09 10 10 10 32 54 76 98

- No.: 1659
- Timestamp: 17:11:49:550_0
- RFN: 7727
- Chip: 30208
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: tc_12_4_1_4c2:lt_Attach_Steps_3To4 LINE 5
- Message Structure:
RRC_DataInd
. (IntegerType)cellId[0] = -1
. (SS_RB_Identity)rB_Id[0] = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain[0] = 1
. (START_Value)start[0] = -
. ATTACHCOMPLETE
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)gMMProtocolDiscriminator[4] = '1000'B
. . (MsgType)msgType[8] = '00000011'B
- Constraint:
car_PS_UplinkDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 08 03

- No.: 1667
- Timestamp: 17:11:49:551_3
- RFN: 7727
- Chip: 34560
- Event: Start Timer
- Source: ts_RRC_Delay LINE 1
- Message Structure:
no details available
- Constraint:
t_Dly (1000 Ms)
- BinaryMessage:

- No.: 1671
- Timestamp: 17:11:50:547_0
- RFN: 7827
- Chip: 20992
- Event: Timeout
- Source: ts_RRC_Delay LINE 2
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 1676
- Timestamp: 17:11:50:548_2
- RFN: 7827
- Chip: 25856
- Event: Send
- PCO: UM
- Message: RLC_UM_DATA_REQ
- Source: ts_RRC_ConnRel:lt_Send_RRC_ConnectionRelease LINE 3
- Message Structure:
RLC_UM_DATA_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 1
. uM_message
. . DL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00000000000000000000000000000000"
. . . . (IntegerType)rrc_MessageSequenceNumber[-1] = 0
. . . DL_DCCH_MessageType
. . . . RRCConnectionRelease
. . . . . r3
. . . . . . RRCConnectionRelease_r3_IEs
. . . . . . . (IntegerType)rrc_TransactionIdentifier[-1] = 0
. . . . . . . (IntegerType)n_308[-1] = 1
. . . . . . . (ReleaseCause)releaseCause[0] = 0
. . . . . . . Rplmn_Information
. . . . . . laterNonCriticalExtensions
. (BooleanType)specialLI = FALSE
- Constraint:
cas_RRC_ConnRelDCCH
- BinaryMessage:
30 10 02 01 ff 02 01 01 80 00 00 00 03 c8 00 01 01 00

- No.: 1680
- Timestamp: 17:11:50:670_0
- RFN: 7839
- Chip: 30464
- Event: Receive
- PCO: UM
- Message: RLC_UM_DATA_IND
- Source: ts_RRC_ConnRel:lt_Send_RRC_ConnectionRelease LINE 4
- Message Structure:
RLC_UM_DATA_IND
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 1
. IntegrityResult
. uM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00100111010100110001100010101000"
. . . . (IntegerType)rrc_MessageSequenceNumber[4] = 1
. . . UL_DCCH_MessageType
. . . . RRCConnectionReleaseComplete
. . . . . (IntegerType)rrc_TransactionIdentifier[2] = 0
. . . . . FailureCauseWithProtErr
. . . . . laterNonCriticalExtensions
- Constraint:
car_RRC_ConnRelCmplUM
- BinaryMessage:
30 0e 02 01 ff 02 01 01 05 00 93 a9 8c 54 0c 40

- No.: 1681
- Timestamp: 17:11:50:671_0
- RFN: 7839
- Chip: 31744
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ConnRel:lt_Send_RRC_ConnectionRelease LINE 4
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1684
- Timestamp: 17:11:50:671_3
- RFN: 7839
- Chip: 33280
- Event: Start Timer
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 1
- Message Structure:
no details available
- Constraint:
t_Dly (5000 Ms)
- BinaryMessage:

- No.: 1688
- Timestamp: 17:11:50:830_0
- RFN: 7855
- Chip: 30208
- Event: Receive
- PCO: UM
- Message: RLC_UM_DATA_IND
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 4
- Message Structure:
RLC_UM_DATA_IND
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 1
. IntegrityResult
. uM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "01100001101000101010011110101100"
. . . . (IntegerType)rrc_MessageSequenceNumber[4] = 2
. . . UL_DCCH_MessageType
. . . . RRCConnectionReleaseComplete
. . . . . (IntegerType)rrc_TransactionIdentifier[2] = 0
. . . . . FailureCauseWithProtErr
. . . . . laterNonCriticalExtensions
- Constraint:
car_RRC_ConnRelCmplUM
- BinaryMessage:
30 0e 02 01 ff 02 01 01 05 00 b0 d1 53 d6 14 40

- No.: 1690
- Timestamp: 17:11:50:830_2
- RFN: 7855
- Chip: 32000
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 4
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1696
- Timestamp: 17:11:50:831_4
- RFN: 7855
- Chip: 37120
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 1
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 01 0a 01 00 05 00

- No.: 1700
- Timestamp: 17:11:50:837_0
- RFN: 7856
- Chip: 18688
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 1703
- Timestamp: 17:11:50:837_3
- RFN: 7856
- Chip: 21760
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 2
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 02 0a 01 00 05 00

- No.: 1707
- Timestamp: 17:11:50:841_0
- RFN: 7856
- Chip: 36096
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 1710
- Timestamp: 17:11:50:842_0
- RFN: 7857
- Chip: 512
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 3
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 03 0a 01 00 05 00

- No.: 1714
- Timestamp: 17:11:50:848_0
- RFN: 7857
- Chip: 25344
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 3
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 1717
- Timestamp: 17:11:50:849_2
- RFN: 7857
- Chip: 28160
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 4
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 04 0a 01 00 05 00

- No.: 1721
- Timestamp: 17:11:50:856_0
- RFN: 7858
- Chip: 17664
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 4
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 1724
- Timestamp: 17:11:50:858_0
- RFN: 7858
- Chip: 23808
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 1
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 136
. . . . . UL_RLC_Mode
. . . . . . UL_UM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (NoExplicitDiscard)timerBasedNoExplicit[0] = 9
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 1
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 1
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_UM_Info
- BinaryMessage:
30 22 02 01 ff 02 01 01 0a 01 00 30 17 30 0d 05 00 30 09 02 02 00 88 30 03 0a 01 09 30 06 02 01 01 02 01 01

- No.: 1728
- Timestamp: 17:11:50:866_0
- RFN: 7859
- Chip: 15616
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 1729
- Timestamp: 17:11:50:868_0
- RFN: 7859
- Chip: 22784
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 3
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 2
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 2
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 2
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 02 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 13 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 02 02 01 02

- No.: 1733
- Timestamp: 17:11:50:880_0
- RFN: 7860
- Chip: 30976
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 4
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 1734
- Timestamp: 17:11:50:881_0
- RFN: 7860
- Chip: 37632
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 5
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 3
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 3
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 3
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 03 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 13 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 03 02 01 03

- No.: 1738
- Timestamp: 17:11:50:898_0
- RFN: 7862
- Chip: 21760
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 6
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 3
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 1739
- Timestamp: 17:11:50:900_0
- RFN: 7862
- Chip: 28416
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 7
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 4
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 4
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 4
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 04 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 13 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 04 02 01 04

- No.: 1743
- Timestamp: 17:11:50:917_0
- RFN: 7864
- Chip: 16640
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 8
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 4
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 1767
- Timestamp: 17:11:50:920_2
- RFN: 7864
- Chip: 28160
- Event: Start Timer
- Source: tc_12_4_1_4c2:lt_TestBody LINE 5
- Message Structure:
no details available
- Constraint:
t_UpperBound (396000 Ms)
- BinaryMessage:

- No.: 1768
- Timestamp: 17:11:50:920_3
- RFN: 7864
- Chip: 28672
- Event: Start Timer
- Source: tc_12_4_1_4c2:lt_TestBody LINE 5
- Message Structure:
no details available
- Constraint:
t_LowerBound (324000 Ms)
- BinaryMessage:

- No.: 1780
- Timestamp: 17:17:14:908_1
- RFN: 40266
- Chip: 25600
- Event: Timeout
- Source: tc_12_4_1_4c2:lt_RARej LINE 1
- Message Structure:
no details available
- Constraint:
t_LowerBound
- BinaryMessage:

- No.: 1784
- Timestamp: 17:17:51:179_0
- RFN: 43894
- Chip: 3072
- Event: Receive
- PCO: TM
- Message: RLC_TR_DATA_IND
- Source: tc_12_4_1_4c2:lt_RARej LINE 2
- Message Structure:
RLC_TR_DATA_IND
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 0
. tM_message
. . UL_CCCH_Message
. . . IntegrityCheckInfo
. . . UL_CCCH_MessageType
. . . . RRCConnectionRequest
. . . . . InitialUE_Identity
. . . . . . P_TMSI_and_RAI_GSM_MAP
. . . . . . . (BitStringType)p_TMSI[32] = "00001001100001110110010101000011"
. . . . . . . RAI
. . . . . . . . LAI
. . . . . . . . . PLMN_Identity
. . . . . . . . . . MCC
. . . . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . . . (IntegerType)_elem[4] = 1
. . . . . . . . . . MNC
. . . . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . . . (IntegerType)_elem[4] = 1
. . . . . . . . . (BitStringType)lac[16] = '0000000000000001'B
. . . . . . . . (BitStringType)rac[8] = "00000101"
. . . . . (EstablishmentCause)establishmentCause[5] = 12
. . . . . (ProtocolErrorIndicator)protocolErrorIndicator[1] = 0
. . . . . MeasuredResultsOnRACH
. . . . . v3d0NonCriticalExtensions
- Constraint:
car_RRC_ConnReq
- BinaryMessage:
30 12 02 01 00 02 01 00 22 09 87 65 43 00 10 08 00 08 2b 00

- No.: 1786
- Timestamp: 17:17:51:180_1
- RFN: 43894
- Chip: 5376
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: tc_12_4_1_4c2:lt_RARej LINE 2
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1801
- Timestamp: 17:17:51:192_0
- RFN: 43895
- Chip: 13312
- Event: Send
- PCO: UM
- Message: RLC_UM_DATA_REQ
- Source: ts_RRC_ConnEstEnd:lt_Send_ConnSetUp LINE 22
- Message Structure:
RLC_UM_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 0
. uM_message
. . DL_CCCH_Message
. . . IntegrityCheckInfo
. . . DL_CCCH_MessageType
. . . . RRCConnectionSetup
. . . . . r3
. . . . . . RRCConnectionSetup_r3_IEs
. . . . . . . InitialUE_Identity
. . . . . . . . P_TMSI_and_RAI_GSM_MAP
. . . . . . . . . (BitStringType)p_TMSI[32] = "00001001100001110110010101000011"
. . . . . . . . . RAI
. . . . . . . . . . LAI
. . . . . . . . . . . PLMN_Identity
. . . . . . . . . . . . MCC
. . . . . . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . . . . . (IntegerType)_elem[4] = 1
. . . . . . . . . . . . MNC
. . . . . . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . . . . . (IntegerType)_elem[4] = 1
. . . . . . . . . . . (BitStringType)lac[16] = '0000000000000001'B
. . . . . . . . . . (BitStringType)rac[8] = "00000101"
. . . . . . . (IntegerType)rrc_TransactionIdentifier[-1] = 0
. . . . . . . (IntegerType)activationTime[-1] = -
. . . . . . . U_RNTI
. . . . . . . . (BitStringType)srnc_Identity[12] = "000000000001"
. . . . . . . . (BitStringType)s_RNTI[20] = "00000000000000000001"
. . . . . . . (BitStringType)new_c_RNTI[16] = -
. . . . . . . (RRC_StateIndicator)rrc_StateIndicator[0] = 0
. . . . . . . (IntegerType)utran_DRX_CycleLengthCoeff[-1] = 9
. . . . . . . CapabilityUpdateRequirement
. . . . . . . . (BooleanType)ue_RadioCapabilityFDDUpdateRequirement = TRUE
. . . . . . . . (BooleanType)ue_RadioCapabilityTDDUpdateRequirement = FALSE
. . . . . . . . SystemSpecificCapUpdateReqList
. . . . . . . . . (SystemSpecificCapUpdateReq)_elem[0] = 0
. . . . . . . SRB_InformationSetupList2
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity[-1] = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_UM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 1
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex[-1] = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 1
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity[-1] = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 2
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 2
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 2
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 2
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex[-1] = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 2
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 2
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity[-1] = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 3
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 3
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 3
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 3
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex[-1] = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 3
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 3
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity[-1] = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 4
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 4
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 4
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 4
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex[-1] = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 4
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 4
. . . . . . . UL_CommonTransChInfo
. . . . . . . . TFC_Subset
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . TFCS
. . . . . . . . . . . ExplicitTFCS_Configuration
. . . . . . . . . . . . TFCS_ReconfAdd
. . . . . . . . . . . . . ctfcSize
. . . . . . . . . . . . . . ctfc2Bit
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . . . . . . . (IntegerType)ctfc2[-1] = 0
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . . . . . . . (IntegerType)ctfc2[-1] = 1
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC[-1] = 11
. . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaD[-1] = 15
. . . . . . . . . . . . . . . . . . . (IntegerType)referenceTFC_ID[-1] = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . UL_AddReconfTransChInfoList
. . . . . . . . UL_AddReconfTransChInformation
. . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType[0] = 0
. . . . . . . . . (IntegerType)transportChannelIdentity[-1] = 5
. . . . . . . . . TransportFormatSet
. . . . . . . . . . DedicatedTransChTFS
. . . . . . . . . . . tti
. . . . . . . . . . . . DedicatedDynamicTF_InfoList
. . . . . . . . . . . . . DedicatedDynamicTF_Info
. . . . . . . . . . . . . . rlc_Size
. . . . . . . . . . . . . . . BitModeRLC_SizeInfo
. . . . . . . . . . . . . . . . sizeType2
. . . . . . . . . . . . . . . . . (IntegerType)part1[-1] = 2
. . . . . . . . . . . . . . . . . (IntegerType)part2[-1] = -
. . . . . . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . LogicalChannelList
. . . . . . . . . . . SemistaticTF_Information
. . . . . . . . . . . . ChannelCodingType
. . . . . . . . . . . . . (CodingRate)convolutional[0] = 1
. . . . . . . . . . . . (IntegerType)rateMatchingAttribute[-1] = 192
. . . . . . . . . . . . (CRC_Size)crc_Size[0] = 3
. . . . . . . DL_CommonTransChInfo
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . dl_Parameters
. . . . . . . DL_AddReconfTransChInfoList
. . . . . . . . DL_AddReconfTransChInformation
. . . . . . . . . (DL_TrCH_Type)dl_TransportChannelType[0] = 0
. . . . . . . . . (IntegerType)dl_transportChannelIdentity[-1] = 10
. . . . . . . . . tfs_SignallingMode
. . . . . . . . . . UL_TransportChannelIdentity
. . . . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType[0] = 0
. . . . . . . . . . . (IntegerType)ul_TransportChannelIdentity[-1] = 5
. . . . . . . . . QualityTarget
. . . . . . . . . . (IntegerType)bler_QualityValue[-1] = -20
. . . . . . . . . TM_SignallingInfo
. . . . . . . FrequencyInfo
. . . . . . . (IntegerType)maxAllowedUL_TX_Power[-1] = -
. . . . . . . UL_ChannelRequirement
. . . . . . . . UL_DPCH_Info
. . . . . . . . . UL_DPCH_PowerControlInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (IntegerType)dpcch_PowerOffset[-1] = -40
. . . . . . . . . . . (IntegerType)pc_Preamble[-1] = 1
. . . . . . . . . . . (IntegerType)sRB_delay[-1] = 7
. . . . . . . . . . . PowerControlAlgorithm
. . . . . . . . . . . . (IntegerType)algorithm1[-1] = 1
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (ScramblingCodeType)scramblingCodeType[0] = 1
. . . . . . . . . . . (IntegerType)scramblingCode[-1] = 0
. . . . . . . . . . . (IntegerType)numberOfDPDCH[-1] = -
. . . . . . . . . . . (SpreadingFactor)spreadingFactor[0] = 4
. . . . . . . . . . . (BooleanType)tfci_Existence = TRUE
. . . . . . . . . . . (IntegerType)numberOfFBI_Bits[-1] = -
. . . . . . . . . . . (PuncturingLimit)puncturingLimit[0] = 15
. . . . . . . DL_CommonInformation
. . . . . . . . DL_DPCH_InfoCommon
. . . . . . . . . cfnHandling
. . . . . . . . . . initialise
. . . . . . . . . . . (IntegerType)cfntargetsfnframeoffset[-1] = -
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . DL_DPCH_PowerControlInfo
. . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . (DPC_Mode)dpc_Mode[0] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPilot_pdpdch[-1] = 0
. . . . . . . . . . . Dl_rate_matching_restriction
. . . . . . . . . . . SF512_AndPilot
. . . . . . . . . . . . (PilotBits128)sfd128[0] = 0
. . . . . . . . . . . (PositionFixedOrFlexible)positionFixedOrFlexible[0] = 0
. . . . . . . . . . . (BooleanType)tfci_Existence = FALSE
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . (IntegerType)defaultDPCH_OffsetValue[-1] = 459
. . . . . . . . . . DPCH_CompressedModeInfo
. . . . . . . . . . (TX_DiversityMode)tx_DiversityMode[0] = 0
. . . . . . . . . . SSDT_Information
. . . . . . . DL_InformationPerRL_List
. . . . . . . . DL_InformationPerRL
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . PrimaryCPICH_Info
. . . . . . . . . . . . (IntegerType)primaryScramblingCode[-1] = 100
. . . . . . . . . . . PDSCH_SHO_DCH_Info
. . . . . . . . . . . PDSCH_CodeMapping
. . . . . . . . . DL_DPCH_InfoPerRL
. . . . . . . . . . fdd
. . . . . . . . . . . (PCPICH_UsageForChannelEst)pCPICH_UsageForChannelEst[0] = 0
. . . . . . . . . . . (IntegerType)dpch_FrameOffset[-1] = 18
. . . . . . . . . . . SecondaryCPICH_Info
. . . . . . . . . . . DL_ChannelisationCodeList
. . . . . . . . . . . . DL_ChannelisationCode
. . . . . . . . . . . . . (IntegerType)secondaryScramblingCode[-1] = 1
. . . . . . . . . . . . . SF512_AndCodeNumber
. . . . . . . . . . . . . . (IntegerType)sf128[-1] = 0
. . . . . . . . . . . . . (ScramblingCodeChange)scramblingCodeChange[0] = 1
. . . . . . . . . . . (IntegerType)tpc_CombinationIndex[-1] = 0
. . . . . . . . . . . (SSDT_CellIdentity)ssdt_CellIdentity[0] = -
. . . . . . . . . . . (ClosedLoopTimingAdjMode)closedLoopTimingAdjMode[0] = -
. . . . . . . . . SCCPCH_InfoForFACH
. . . . . . laterNonCriticalExtensions
. (BooleanType)specialLI = TRUE
- Constraint:
cas_RRC_ConnSetup
- BinaryMessage:
30 79 02 01 00 02 01 00 30 e7 41 30 ec a8 60 02 01 00 01 05 00 04 00 00 4d 82 69 3a 10 10 89 0d 42 00 02 81 9e 8e 46 c9 a6 7c 9c 4e 74 20 a5 12 3a 8c 00 15 13 3d 1c 8d 93 4c f9 38 9c e8 42 52 24 b5 28 00 4a 46 7a 39 1b 26 99 f2 71 39 d0 86 b4 49 ea 70 00 d4 c8 00 06 25 2b f0 02 00 08 82 23 bf 66 08 98 95 a5 47 a2 00 00 01 3f 90 0a 14 e5 82 06 40 09 0c 28 08 01 01 ff

- No.: 1822
- Timestamp: 17:17:51:215_3
- RFN: 43897
- Chip: 25088
- Event: Start Timer
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 3
- Message Structure:
no details available
- Constraint:
t_WaitMS (13500 Ms)
- BinaryMessage:

- No.: 1824
- Timestamp: 17:17:51:215_5
- RFN: 43897
- Chip: 27136
- Event: Receive
- PCO: CPHY
- Message: CPHY_Out_of_Sync_IND
- Source: RRC_DefConnEst LINE 7
- Message Structure:
CPHY_Out_of_Sync_IND
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 20
- Constraint:
ca_OutOfSyncInd
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 1826
- Timestamp: 17:17:51:216_1
- RFN: 43897
- Chip: 28672
- Event: Default
- Source: RRC_DefConnEst LINE 0
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1827
- Timestamp: 17:17:51:216_2
- RFN: 43897
- Chip: 28928
- Event: Default
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1835
- Timestamp: 17:17:51:416_1
- RFN: 43917
- Chip: 29184
- Event: Receive
- PCO: CPHY
- Message: CPHY_Sync_IND
- Source: RRC_DefConnEst LINE 5
- Message Structure:
CPHY_Sync_IND
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 20
- Constraint:
ca_SyncInd
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 1837
- Timestamp: 17:17:51:417_1
- RFN: 43917
- Chip: 30464
- Event: Default
- Source: RRC_DefConnEst LINE 0
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1838
- Timestamp: 17:17:51:417_2
- RFN: 43917
- Chip: 30976
- Event: Default
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1845
- Timestamp: 17:17:51:538_0
- RFN: 43929
- Chip: 37120
- Event: Receive
- PCO: AM
- Message: RLC_AM_DATA_IND
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
RLC_AM_DATA_IND
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 2
. IntegrityResult
. . (IntegrityStatus)integrityUsed[0] = 4294967296
. aM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . UL_DCCH_MessageType
. . . . RRCConnectionSetupComplete
. . . . . (IntegerType)rrc_TransactionIdentifier[2] = 0
. . . . . STARTList
. . . . . . STARTSingle
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity[1] = 0
. . . . . . . (BitStringType)start_Value[20] = "11111111111111111111"
. . . . . . STARTSingle
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity[1] = 1
. . . . . . . (BitStringType)start_Value[20] = "00000000000000000010"
. . . . . UE_RadioAccessCapability
. . . . . . (AccessStratumReleaseIndicator)accessStratumReleaseIndicator[0] = 0
. . . . . . PDCP_Capability
. . . . . . . (BooleanType)losslessSRNS_RelocationSupport = TRUE
. . . . . . . supportForRfc2507
. . . . . . RLC_Capability
. . . . . . . (TotalRLC_AM_BufferSize)totalRLC_AM_BufferSize[3] = 2
. . . . . . . (MaximumRLC_WindowSize)maximumRLC_WindowSize[1] = 0
. . . . . . . (MaximumAM_EntityNumberRLC_Cap)maximumAM_EntityNumber[3] = 3
. . . . . . TransportChannelCapability
. . . . . . . DL_TransChCapability
. . . . . . . . (MaxNoBits)maxNoBitsReceived[4] = 4
. . . . . . . . (MaxNoBits)maxConvCodeBitsReceived[4] = 0
. . . . . . . . TurboSupport
. . . . . . . . . (MaxNoBits)supported[4] = 4
. . . . . . . . (MaxSimultaneousTransChsDL)maxSimultaneousTransChs[2] = 1
. . . . . . . . (IntegerType)maxSimultaneousCCTrCH_Count[3] = 1
. . . . . . . . (MaxTransportBlocksDL)maxReceivedTransportBlocks[4] = 3
. . . . . . . . (MaxNumberOfTFC_DL)maxNumberOfTFC[4] = 5
. . . . . . . . (MaxNumberOfTF)maxNumberOfTF[3] = 1
. . . . . . . UL_TransChCapability
. . . . . . . . (MaxNoBits)maxNoBitsTransmitted[4] = 3
. . . . . . . . (MaxNoBits)maxConvCodeBitsTransmitted[4] = 0
. . . . . . . . TurboSupport
. . . . . . . . . (MaxNoBits)supported[4] = 3
. . . . . . . . (MaxSimultaneousTransChsUL)maxSimultaneousTransChs[3] = 2
. . . . . . . . modeSpecificInfo
. . . . . . . . (MaxTransportBlocksUL)maxTransmittedBlocks[4] = 2
. . . . . . . . (MaxNumberOfTFC_UL)maxNumberOfTFC[4] = 3
. . . . . . . . (MaxNumberOfTF)maxNumberOfTF[3] = 0
. . . . . . RF_Capability
. . . . . . . fddRF_Capability
. . . . . . . tddRF_Capability
. . . . . . PhysicalChannelCapability
. . . . . . . fddPhysChCapability
. . . . . . . . DL_PhysChCapabilityFDD
. . . . . . . . . (IntegerType)maxNoDPCH_PDSCH_Codes[3] = 3
. . . . . . . . . (MaxNoPhysChBitsReceived)maxNoPhysChBitsReceived[4] = 6
. . . . . . . . . (BooleanType)supportForSF_512 = FALSE
. . . . . . . . . (BooleanType)supportOfPDSCH = FALSE
. . . . . . . . . SimultaneousSCCPCH_DPCH_Reception
. . . . . . . . UL_PhysChCapabilityFDD
. . . . . . . . . (MaxNoDPDCH_BitsTransmitted)maxNoDPDCH_BitsTransmitted[4] = 2
. . . . . . . . . (BooleanType)supportOfPCPCH = FALSE
. . . . . . . tddPhysChCapability
. . . . . . UE_MultiModeRAT_Capability
. . . . . . . MultiRAT_Capability
. . . . . . . . (BooleanType)supportOfGSM = FALSE
. . . . . . . . (BooleanType)supportOfMulticarrier = FALSE
. . . . . . . (MultiModeCapability)multiModeCapability[2] = 1
. . . . . . SecurityCapability
. . . . . . . (BitStringType)cipheringAlgorithmCap[16] = '0000000000000001'B
. . . . . . . (BitStringType)integrityProtectionAlgorithmCap[16] = '0000000000000010'B
. . . . . . UE_Positioning_Capability
. . . . . . . (BooleanType)standaloneLocMethodsSupported = FALSE
. . . . . . . (BooleanType)ue_BasedOTDOA_Supported = FALSE
. . . . . . . (NetworkAssistedGPS_Supported)networkAssistedGPS_Supported[2] = 1
. . . . . . . (BooleanType)supportForUE_GPS_TimingOfCellFrames = FALSE
. . . . . . . (BooleanType)supportForIPDL = FALSE
. . . . . . MeasurementCapability
. . . . . v370NonCriticalExtensions
. . . . . . RRCConnectionSetupComplete_v370ext
. . . . . . . UE_RadioAccessCapability_v370ext
. . . . . . . . UE_RadioAccessCapabBandFDDList
. . . . . . . . . UE_RadioAccessCapabBandFDD
. . . . . . . . . . (RadioFrequencyBandFDD)radioFrequencyBandFDD[3] = 1
. . . . . . . . . . fddRF_Capability
. . . . . . . . . . . (UE_PowerClassExt)ue_PowerClass[3] = 3
. . . . . . . . . . . (TxRxFrequencySeparation)txRxFrequencySeparation[2] = 0
. . . . . . . . . . MeasurementCapabilityExt
. . . . . . . . . . . CompressedModeMeasCapabFDDList
. . . . . . . . . . . . CompressedModeMeasCapabFDD
. . . . . . . . . . . . . (RadioFrequencyBandFDD)radioFrequencyBandFDD[3] = 1
. . . . . . . . . . . . . (BooleanType)dl_MeasurementsFDD = TRUE
. . . . . . . . . . . . . (BooleanType)ul_MeasurementsFDD = TRUE
. . . . . . . . . . . CompressedModeMeasCapabGSMList
. . . . . . . . . . . . CompressedModeMeasCapabGSM
. . . . . . . . . . . . . (RadioFrequencyBandGSM)radioFrequencyBandGSM[4] = 2
. . . . . . . . . . . . . (BooleanType)dl_MeasurementsGSM = FALSE
. . . . . . . . . . . . . (BooleanType)ul_MeasurementsGSM = FALSE
. . . . . . . . . . . . CompressedModeMeasCapabGSM
. . . . . . . . . . . . . (RadioFrequencyBandGSM)radioFrequencyBandGSM[4] = 6
. . . . . . . . . . . . . (BooleanType)dl_MeasurementsGSM = FALSE
. . . . . . . . . . . . . (BooleanType)ul_MeasurementsGSM = TRUE
. . . . . . . . . . . CompressedModeMeasCapabMC
. . . . . . v380NonCriticalExtensions
- Constraint:
car_RRC_ConnSetupCmpl
- BinaryMessage:
30 2a 02 01 ff 02 01 02 0a 05 01 00 00 00 00 4a 8b ff ff e0 00 04 91 a0 51 06 a4 c2 68 46 09 30 20 80 00 80 01 08 89 62 13 89 0c 80

- No.: 1847
- Timestamp: 17:17:51:540_1
- RFN: 43930
- Chip: 6656
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1865
- Timestamp: 17:17:51:676_0
- RFN: 43943
- Chip: 32768
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: tc_12_4_1_4c2:lt_RARej LINE 4
- Message Structure:
RRC_DataInd
. (IntegerType)cellId[0] = -1
. (SS_RB_Identity)rB_Id[0] = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain[0] = 1
. (START_Value)start[20] = '00000000000000000010'B
. ROUTINGAREAUPDATEREQUEST
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)gMMProtocolDiscriminator[4] = '1000'B
. . (MsgType)msgType[8] = '00001000'B
. . CiphKeySeqNum
. . . (B1)spare1[1] = '0'B
. . . (KeySeq)keySeq[3] = '001'B
. . UpdateType_v
. . . (B1)pre_for[1] = '0'B
. . . (B3)value[3] = '011'B
. . RAI_v
. . . (OctetStringType)plmn[3] = '00F110'O
. . . (OctetStringType)lac[2] = '0001'O
. . . (OctetStringType)rac[1] = '05'O
. . MSRadioAccessCap_lv
. . . (Length)iel[1] = '05'O
. . . (OctetStringType)value[5] = '02C2000600'O
. . PTMSI_Signature
. . . (IEI8)iei[8] = '00011001'B
. . . (OctetStringType)value[3] = 'AB1237'O
. . GPRS_Timer
. . . (IEI8)iei[8] = '00010111'B
. . . (B3)unit[3] = '000'B
. . . (B5)value[5] = '11110'B
. . DRXparamter_tv
. . TMSI_Status
. . GMM_MS_IdentityPTMSI
. . . (IEI8)iei[8] = '00011000'B
. . . (Length)iel[1] = '05'O
. . . (B4)iDigit1[4] = '1111'B
. . . (B1)oddEvenInd[1] = '0'B
. . . (B3)typeOfId[3] = '100'B
. . . (OctetStringType)otherDigits[4] = '09876543'O
. . MS_NetworkCap_tlv
. . . (IEI8)iei[8] = '00110001'B
. . . (Length)iel[1] = '02'O
. . . (OctetStringType)value[2] = 'C500'O
. . PDP_ContextStatus
. . . (IEI8)iei[0] = -
. . . (Length)iel[1] = -
. . . (BitStringType)nSAPI[0] = -
- Constraint:
car_PS_InitDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 03 04 04 00 00 20 08 08 13 00 f1 10 00 01 05 05 02 c2 00 06 00 19 ab 12 37 17 1e 18 05 f4 09 87 65 43 31 02 c5 00

- No.: 1870
- Timestamp: 17:17:51:678_0
- RFN: 43944
- Chip: 768
- Event: Send
- PCO: Dc
- Message: RRC_DataReq
- Source: tc_12_4_1_4c2:lt_RARej LINE 6
- Message Structure:
RRC_DataReq
. (IntegerType)cellId[-1] = -1
. (SS_RB_Identity)rB_Id[-1] = 3
. (LogicChGERAN)ch[-1] = -
. (SapId)sapId[1] = -
. (SS_CN_DomainIdentity)cN_Domain[-1] = 1
. ROUTING_AREA_UPDATE_REJECT
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)gMMProtocolDiscriminator[4] = '1000'B
. . (MsgType)msgType[8] = '00001011'B
. . (RejCau)gmmCause[1] = '0E'O
. . (B4)spare[4] = '0000'B
. . ForceToStandby
. . . (B1)spare[1] = '0'B
. . . (B3)value[3] = '000'B
. . GPRS_Timer
- Constraint:
ca_PS_DataReq
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 08 0b 0e 00

- No.: 1879
- Timestamp: 17:17:51:679_6
- RFN: 43944
- Chip: 5376
- Event: Start Timer
- Source: ts_RRC_Delay LINE 1
- Message Structure:
no details available
- Constraint:
t_Dly (1000 Ms)
- BinaryMessage:

- No.: 1883
- Timestamp: 17:17:52:673_0
- RFN: 44043
- Chip: 17408
- Event: Timeout
- Source: ts_RRC_Delay LINE 2
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 1888
- Timestamp: 17:17:52:675_0
- RFN: 44043
- Chip: 22784
- Event: Send
- PCO: UM
- Message: RLC_UM_DATA_REQ
- Source: ts_RRC_ConnRel:lt_Send_RRC_ConnectionRelease LINE 3
- Message Structure:
RLC_UM_DATA_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 1
. uM_message
. . DL_DCCH_Message
. . . IntegrityCheckInfo
. . . DL_DCCH_MessageType
. . . . RRCConnectionRelease
. . . . . r3
. . . . . . RRCConnectionRelease_r3_IEs
. . . . . . . (IntegerType)rrc_TransactionIdentifier[-1] = 0
. . . . . . . (IntegerType)n_308[-1] = 1
. . . . . . . (ReleaseCause)releaseCause[0] = 0
. . . . . . . Rplmn_Information
. . . . . . laterNonCriticalExtensions
. (BooleanType)specialLI = FALSE
- Constraint:
cas_RRC_ConnRelDCCH
- BinaryMessage:
30 0c 02 01 ff 02 01 01 3c 80 00 01 01 00

- No.: 1892
- Timestamp: 17:17:52:796_0
- RFN: 44055
- Chip: 29440
- Event: Receive
- PCO: UM
- Message: RLC_UM_DATA_IND
- Source: ts_RRC_ConnRel:lt_Send_RRC_ConnectionRelease LINE 4
- Message Structure:
RLC_UM_DATA_IND
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 1
. IntegrityResult
. uM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . UL_DCCH_MessageType
. . . . RRCConnectionReleaseComplete
. . . . . (IntegerType)rrc_TransactionIdentifier[2] = 0
. . . . . FailureCauseWithProtErr
. . . . . laterNonCriticalExtensions
- Constraint:
car_RRC_ConnRelCmplUM
- BinaryMessage:
30 0a 02 01 ff 02 01 01 05 00 44 00

- No.: 1893
- Timestamp: 17:17:52:796_1
- RFN: 44055
- Chip: 30464
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ConnRel:lt_Send_RRC_ConnectionRelease LINE 4
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1896
- Timestamp: 17:17:52:797_0
- RFN: 44055
- Chip: 32512
- Event: Start Timer
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 1
- Message Structure:
no details available
- Constraint:
t_Dly (5000 Ms)
- BinaryMessage:

- No.: 1900
- Timestamp: 17:17:52:955_0
- RFN: 44071
- Chip: 29440
- Event: Receive
- PCO: UM
- Message: RLC_UM_DATA_IND
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 4
- Message Structure:
RLC_UM_DATA_IND
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 1
. IntegrityResult
. uM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . UL_DCCH_MessageType
. . . . RRCConnectionReleaseComplete
. . . . . (IntegerType)rrc_TransactionIdentifier[2] = 0
. . . . . FailureCauseWithProtErr
. . . . . laterNonCriticalExtensions
- Constraint:
car_RRC_ConnRelCmplUM
- BinaryMessage:
30 0a 02 01 ff 02 01 01 05 00 44 00

- No.: 1902
- Timestamp: 17:17:52:956_1
- RFN: 44071
- Chip: 31488
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 4
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1908
- Timestamp: 17:17:52:957_1
- RFN: 44071
- Chip: 36608
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 1
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 01 0a 01 00 05 00

- No.: 1912
- Timestamp: 17:17:52:962_0
- RFN: 44072
- Chip: 17920
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 1915
- Timestamp: 17:17:52:963_2
- RFN: 44072
- Chip: 20992
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 2
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 02 0a 01 00 05 00

- No.: 1919
- Timestamp: 17:17:52:967_0
- RFN: 44072
- Chip: 35328
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 1922
- Timestamp: 17:17:52:968_0
- RFN: 44072
- Chip: 38144
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 3
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 03 0a 01 00 05 00

- No.: 1926
- Timestamp: 17:17:52:974_0
- RFN: 44073
- Chip: 25856
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 3
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 1929
- Timestamp: 17:17:52:975_2
- RFN: 44073
- Chip: 29440
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 4
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 04 0a 01 00 05 00

- No.: 1933
- Timestamp: 17:17:52:983_0
- RFN: 44074
- Chip: 16896
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 4
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 1936
- Timestamp: 17:17:52:985_0
- RFN: 44074
- Chip: 23296
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 1
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 136
. . . . . UL_RLC_Mode
. . . . . . UL_UM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (NoExplicitDiscard)timerBasedNoExplicit[0] = 9
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 1
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 1
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_UM_Info
- BinaryMessage:
30 22 02 01 ff 02 01 01 0a 01 00 30 17 30 0d 05 00 30 09 02 02 00 88 30 03 0a 01 09 30 06 02 01 01 02 01 01

- No.: 1940
- Timestamp: 17:17:52:989_0
- RFN: 44075
- Chip: 0
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 1941
- Timestamp: 17:17:52:990_0
- RFN: 44075
- Chip: 6144
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 3
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 2
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 2
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 2
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 02 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 13 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 02 02 01 02

- No.: 1945
- Timestamp: 17:17:53:004_0
- RFN: 44076
- Chip: 20736
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 4
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 1946
- Timestamp: 17:17:53:006_0
- RFN: 44076
- Chip: 27392
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 5
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 3
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 3
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 3
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 03 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 13 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 03 02 01 03

- No.: 1950
- Timestamp: 17:17:53:019_0
- RFN: 44078
- Chip: 3072
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 6
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 3
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 1951
- Timestamp: 17:17:53:021_0
- RFN: 44078
- Chip: 9728
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 7
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 4
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 4
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 4
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 04 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 13 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 04 02 01 04

- No.: 1955
- Timestamp: 17:17:53:035_0
- RFN: 44079
- Chip: 25600
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 8
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 4
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 1979
- Timestamp: 17:17:53:038_6
- RFN: 44079
- Chip: 37632
- Event: Start Timer
- Source: tc_12_4_1_4c2:lt_LocUpateStep8 LINE 2
- Message Structure:
no details available
- Constraint:
t_UpperBound (396000 Ms)
- BinaryMessage:

- No.: 1980
- Timestamp: 17:17:53:038_7
- RFN: 44080
- Chip: 0
- Event: Start Timer
- Source: tc_12_4_1_4c2:lt_LocUpateStep8 LINE 2
- Message Structure:
no details available
- Constraint:
t_LowerBound (324000 Ms)
- BinaryMessage:

- No.: 1987
- Timestamp: 17:23:17:026_0
- RFN: 76481
- Chip: 33536
- Event: Timeout
- Source: tc_12_4_1_4c2:lt_LocUpateStep8 LINE 3
- Message Structure:
no details available
- Constraint:
t_LowerBound
- BinaryMessage:

- No.: 1991
- Timestamp: 17:23:39:153_0
- RFN: 78694
- Chip: 27904
- Event: Receive
- PCO: TM
- Message: RLC_TR_DATA_IND
- Source: tc_12_4_1_4c2:lt_LocUpateStep8 LINE 4
- Message Structure:
RLC_TR_DATA_IND
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 0
. tM_message
. . UL_CCCH_Message
. . . IntegrityCheckInfo
. . . UL_CCCH_MessageType
. . . . RRCConnectionRequest
. . . . . InitialUE_Identity
. . . . . . IMSI_GSM_MAP
. . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . (IntegerType)_elem[4] = 1
. . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . (IntegerType)_elem[4] = 1
. . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . (IntegerType)_elem[4] = 1
. . . . . . . (IntegerType)_elem[4] = 2
. . . . . . . (IntegerType)_elem[4] = 3
. . . . . . . (IntegerType)_elem[4] = 4
. . . . . . . (IntegerType)_elem[4] = 5
. . . . . . . (IntegerType)_elem[4] = 6
. . . . . . . (IntegerType)_elem[4] = 7
. . . . . . . (IntegerType)_elem[4] = 8
. . . . . . . (IntegerType)_elem[4] = 9
. . . . . (EstablishmentCause)establishmentCause[5] = 12
. . . . . (ProtocolErrorIndicator)protocolErrorIndicator[1] = 0
. . . . . MeasuredResultsOnRACH
. . . . . v3d0NonCriticalExtensions
- Constraint:
car_RRC_ConnReq
- BinaryMessage:
30 10 02 01 00 02 01 00 20 90 01 01 01 23 45 67 89 60

- No.: 1993
- Timestamp: 17:23:39:154_1
- RFN: 78694
- Chip: 30208
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: tc_12_4_1_4c2:lt_LocUpateStep8 LINE 4
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2008
- Timestamp: 17:23:39:164_0
- RFN: 78695
- Chip: 32000
- Event: Send
- PCO: UM
- Message: RLC_UM_DATA_REQ
- Source: ts_RRC_ConnEstEnd:lt_Send_ConnSetUp LINE 22
- Message Structure:
RLC_UM_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 0
. uM_message
. . DL_CCCH_Message
. . . IntegrityCheckInfo
. . . DL_CCCH_MessageType
. . . . RRCConnectionSetup
. . . . . r3
. . . . . . RRCConnectionSetup_r3_IEs
. . . . . . . InitialUE_Identity
. . . . . . . . IMSI_GSM_MAP
. . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . (IntegerType)_elem[4] = 1
. . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . (IntegerType)_elem[4] = 1
. . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . (IntegerType)_elem[4] = 1
. . . . . . . . . (IntegerType)_elem[4] = 2
. . . . . . . . . (IntegerType)_elem[4] = 3
. . . . . . . . . (IntegerType)_elem[4] = 4
. . . . . . . . . (IntegerType)_elem[4] = 5
. . . . . . . . . (IntegerType)_elem[4] = 6
. . . . . . . . . (IntegerType)_elem[4] = 7
. . . . . . . . . (IntegerType)_elem[4] = 8
. . . . . . . . . (IntegerType)_elem[4] = 9
. . . . . . . (IntegerType)rrc_TransactionIdentifier[-1] = 0
. . . . . . . (IntegerType)activationTime[-1] = -
. . . . . . . U_RNTI
. . . . . . . . (BitStringType)srnc_Identity[12] = "000000000001"
. . . . . . . . (BitStringType)s_RNTI[20] = "00000000000000000001"
. . . . . . . (BitStringType)new_c_RNTI[16] = -
. . . . . . . (RRC_StateIndicator)rrc_StateIndicator[0] = 0
. . . . . . . (IntegerType)utran_DRX_CycleLengthCoeff[-1] = 9
. . . . . . . CapabilityUpdateRequirement
. . . . . . . . (BooleanType)ue_RadioCapabilityFDDUpdateRequirement = TRUE
. . . . . . . . (BooleanType)ue_RadioCapabilityTDDUpdateRequirement = FALSE
. . . . . . . . SystemSpecificCapUpdateReqList
. . . . . . . . . (SystemSpecificCapUpdateReq)_elem[0] = 0
. . . . . . . SRB_InformationSetupList2
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity[-1] = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_UM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 1
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex[-1] = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 1
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity[-1] = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 2
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 2
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 2
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 2
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex[-1] = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 2
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 2
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity[-1] = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 3
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 3
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 3
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 3
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex[-1] = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 3
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 3
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity[-1] = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 4
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 4
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 4
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 4
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex[-1] = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 4
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 4
. . . . . . . UL_CommonTransChInfo
. . . . . . . . TFC_Subset
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . TFCS
. . . . . . . . . . . ExplicitTFCS_Configuration
. . . . . . . . . . . . TFCS_ReconfAdd
. . . . . . . . . . . . . ctfcSize
. . . . . . . . . . . . . . ctfc2Bit
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . . . . . . . (IntegerType)ctfc2[-1] = 0
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . . . . . . . (IntegerType)ctfc2[-1] = 1
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC[-1] = 11
. . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaD[-1] = 15
. . . . . . . . . . . . . . . . . . . (IntegerType)referenceTFC_ID[-1] = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . UL_AddReconfTransChInfoList
. . . . . . . . UL_AddReconfTransChInformation
. . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType[0] = 0
. . . . . . . . . (IntegerType)transportChannelIdentity[-1] = 5
. . . . . . . . . TransportFormatSet
. . . . . . . . . . DedicatedTransChTFS
. . . . . . . . . . . tti
. . . . . . . . . . . . DedicatedDynamicTF_InfoList
. . . . . . . . . . . . . DedicatedDynamicTF_Info
. . . . . . . . . . . . . . rlc_Size
. . . . . . . . . . . . . . . BitModeRLC_SizeInfo
. . . . . . . . . . . . . . . . sizeType2
. . . . . . . . . . . . . . . . . (IntegerType)part1[-1] = 2
. . . . . . . . . . . . . . . . . (IntegerType)part2[-1] = -
. . . . . . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . LogicalChannelList
. . . . . . . . . . . SemistaticTF_Information
. . . . . . . . . . . . ChannelCodingType
. . . . . . . . . . . . . (CodingRate)convolutional[0] = 1
. . . . . . . . . . . . (IntegerType)rateMatchingAttribute[-1] = 192
. . . . . . . . . . . . (CRC_Size)crc_Size[0] = 3
. . . . . . . DL_CommonTransChInfo
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . dl_Parameters
. . . . . . . DL_AddReconfTransChInfoList
. . . . . . . . DL_AddReconfTransChInformation
. . . . . . . . . (DL_TrCH_Type)dl_TransportChannelType[0] = 0
. . . . . . . . . (IntegerType)dl_transportChannelIdentity[-1] = 10
. . . . . . . . . tfs_SignallingMode
. . . . . . . . . . UL_TransportChannelIdentity
. . . . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType[0] = 0
. . . . . . . . . . . (IntegerType)ul_TransportChannelIdentity[-1] = 5
. . . . . . . . . QualityTarget
. . . . . . . . . . (IntegerType)bler_QualityValue[-1] = -20
. . . . . . . . . TM_SignallingInfo
. . . . . . . FrequencyInfo
. . . . . . . (IntegerType)maxAllowedUL_TX_Power[-1] = -
. . . . . . . UL_ChannelRequirement
. . . . . . . . UL_DPCH_Info
. . . . . . . . . UL_DPCH_PowerControlInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (IntegerType)dpcch_PowerOffset[-1] = -40
. . . . . . . . . . . (IntegerType)pc_Preamble[-1] = 1
. . . . . . . . . . . (IntegerType)sRB_delay[-1] = 7
. . . . . . . . . . . PowerControlAlgorithm
. . . . . . . . . . . . (IntegerType)algorithm1[-1] = 1
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (ScramblingCodeType)scramblingCodeType[0] = 1
. . . . . . . . . . . (IntegerType)scramblingCode[-1] = 0
. . . . . . . . . . . (IntegerType)numberOfDPDCH[-1] = -
. . . . . . . . . . . (SpreadingFactor)spreadingFactor[0] = 4
. . . . . . . . . . . (BooleanType)tfci_Existence = TRUE
. . . . . . . . . . . (IntegerType)numberOfFBI_Bits[-1] = -
. . . . . . . . . . . (PuncturingLimit)puncturingLimit[0] = 15
. . . . . . . DL_CommonInformation
. . . . . . . . DL_DPCH_InfoCommon
. . . . . . . . . cfnHandling
. . . . . . . . . . initialise
. . . . . . . . . . . (IntegerType)cfntargetsfnframeoffset[-1] = -
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . DL_DPCH_PowerControlInfo
. . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . (DPC_Mode)dpc_Mode[0] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPilot_pdpdch[-1] = 0
. . . . . . . . . . . Dl_rate_matching_restriction
. . . . . . . . . . . SF512_AndPilot
. . . . . . . . . . . . (PilotBits128)sfd128[0] = 0
. . . . . . . . . . . (PositionFixedOrFlexible)positionFixedOrFlexible[0] = 0
. . . . . . . . . . . (BooleanType)tfci_Existence = FALSE
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . (IntegerType)defaultDPCH_OffsetValue[-1] = 459
. . . . . . . . . . DPCH_CompressedModeInfo
. . . . . . . . . . (TX_DiversityMode)tx_DiversityMode[0] = 0
. . . . . . . . . . SSDT_Information
. . . . . . . DL_InformationPerRL_List
. . . . . . . . DL_InformationPerRL
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . PrimaryCPICH_Info
. . . . . . . . . . . . (IntegerType)primaryScramblingCode[-1] = 100
. . . . . . . . . . . PDSCH_SHO_DCH_Info
. . . . . . . . . . . PDSCH_CodeMapping
. . . . . . . . . DL_DPCH_InfoPerRL
. . . . . . . . . . fdd
. . . . . . . . . . . (PCPICH_UsageForChannelEst)pCPICH_UsageForChannelEst[0] = 0
. . . . . . . . . . . (IntegerType)dpch_FrameOffset[-1] = 18
. . . . . . . . . . . SecondaryCPICH_Info
. . . . . . . . . . . DL_ChannelisationCodeList
. . . . . . . . . . . . DL_ChannelisationCode
. . . . . . . . . . . . . (IntegerType)secondaryScramblingCode[-1] = 1
. . . . . . . . . . . . . SF512_AndCodeNumber
. . . . . . . . . . . . . . (IntegerType)sf128[-1] = 0
. . . . . . . . . . . . . (ScramblingCodeChange)scramblingCodeChange[0] = 1
. . . . . . . . . . . (IntegerType)tpc_CombinationIndex[-1] = 0
. . . . . . . . . . . (SSDT_CellIdentity)ssdt_CellIdentity[0] = -
. . . . . . . . . . . (ClosedLoopTimingAdjMode)closedLoopTimingAdjMode[0] = -
. . . . . . . . . SCCPCH_InfoForFACH
. . . . . . laterNonCriticalExtensions
. (BooleanType)specialLI = TRUE
- Constraint:
cas_RRC_ConnSetup
- BinaryMessage:
30 78 02 01 00 02 01 00 30 e7 12 00 20 20 24 68 ac f1 20 00 80 00 09 b0 4d 27 42 02 11 21 a8 40 00 50 33 d1 c8 d9 34 cf 93 89 ce 84 14 a2 47 51 80 02 a2 67 a3 91 b2 69 9f 27 13 9d 08 4a 44 96 a5 00 09 48 cf 47 23 64 d3 3e 4e 27 3a 10 d6 89 3d 4e 00 1a 99 00 00 c4 a5 7e 00 40 01 10 44 77 ec c1 13 12 b4 a8 f4 40 00 00 27 f2 01 42 9c b0 40 c8 01 21 85 01 00 01 01 ff

- No.: 2029
- Timestamp: 17:23:39:187_3
- RFN: 78698
- Chip: 5120
- Event: Start Timer
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 3
- Message Structure:
no details available
- Constraint:
t_WaitMS (13500 Ms)
- BinaryMessage:

- No.: 2031
- Timestamp: 17:23:39:188_0
- RFN: 78698
- Chip: 7424
- Event: Receive
- PCO: CPHY
- Message: CPHY_Out_of_Sync_IND
- Source: RRC_DefConnEst LINE 7
- Message Structure:
CPHY_Out_of_Sync_IND
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 20
- Constraint:
ca_OutOfSyncInd
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 2033
- Timestamp: 17:23:39:188_2
- RFN: 78698
- Chip: 8960
- Event: Default
- Source: RRC_DefConnEst LINE 0
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2034
- Timestamp: 17:23:39:188_3
- RFN: 78698
- Chip: 9472
- Event: Default
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2042
- Timestamp: 17:23:39:414_0
- RFN: 78720
- Chip: 29952
- Event: Receive
- PCO: CPHY
- Message: CPHY_Sync_IND
- Source: RRC_DefConnEst LINE 5
- Message Structure:
CPHY_Sync_IND
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 20
- Constraint:
ca_SyncInd
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 2044
- Timestamp: 17:23:39:414_2
- RFN: 78720
- Chip: 31232
- Event: Default
- Source: RRC_DefConnEst LINE 0
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2045
- Timestamp: 17:23:39:414_3
- RFN: 78720
- Chip: 31744
- Event: Default
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2052
- Timestamp: 17:23:39:535_0
- RFN: 78732
- Chip: 35584
- Event: Receive
- PCO: AM
- Message: RLC_AM_DATA_IND
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
RLC_AM_DATA_IND
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 2
. IntegrityResult
. . (IntegrityStatus)integrityUsed[0] = 4294967296
. aM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . UL_DCCH_MessageType
. . . . RRCConnectionSetupComplete
. . . . . (IntegerType)rrc_TransactionIdentifier[2] = 0
. . . . . STARTList
. . . . . . STARTSingle
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity[1] = 0
. . . . . . . (BitStringType)start_Value[20] = "11111111111111111111"
. . . . . . STARTSingle
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity[1] = 1
. . . . . . . (BitStringType)start_Value[20] = "00000000000000000010"
. . . . . UE_RadioAccessCapability
. . . . . . (AccessStratumReleaseIndicator)accessStratumReleaseIndicator[0] = 0
. . . . . . PDCP_Capability
. . . . . . . (BooleanType)losslessSRNS_RelocationSupport = TRUE
. . . . . . . supportForRfc2507
. . . . . . RLC_Capability
. . . . . . . (TotalRLC_AM_BufferSize)totalRLC_AM_BufferSize[3] = 2
. . . . . . . (MaximumRLC_WindowSize)maximumRLC_WindowSize[1] = 0
. . . . . . . (MaximumAM_EntityNumberRLC_Cap)maximumAM_EntityNumber[3] = 3
. . . . . . TransportChannelCapability
. . . . . . . DL_TransChCapability
. . . . . . . . (MaxNoBits)maxNoBitsReceived[4] = 4
. . . . . . . . (MaxNoBits)maxConvCodeBitsReceived[4] = 0
. . . . . . . . TurboSupport
. . . . . . . . . (MaxNoBits)supported[4] = 4
. . . . . . . . (MaxSimultaneousTransChsDL)maxSimultaneousTransChs[2] = 1
. . . . . . . . (IntegerType)maxSimultaneousCCTrCH_Count[3] = 1
. . . . . . . . (MaxTransportBlocksDL)maxReceivedTransportBlocks[4] = 3
. . . . . . . . (MaxNumberOfTFC_DL)maxNumberOfTFC[4] = 5
. . . . . . . . (MaxNumberOfTF)maxNumberOfTF[3] = 1
. . . . . . . UL_TransChCapability
. . . . . . . . (MaxNoBits)maxNoBitsTransmitted[4] = 3
. . . . . . . . (MaxNoBits)maxConvCodeBitsTransmitted[4] = 0
. . . . . . . . TurboSupport
. . . . . . . . . (MaxNoBits)supported[4] = 3
. . . . . . . . (MaxSimultaneousTransChsUL)maxSimultaneousTransChs[3] = 2
. . . . . . . . modeSpecificInfo
. . . . . . . . (MaxTransportBlocksUL)maxTransmittedBlocks[4] = 2
. . . . . . . . (MaxNumberOfTFC_UL)maxNumberOfTFC[4] = 3
. . . . . . . . (MaxNumberOfTF)maxNumberOfTF[3] = 0
. . . . . . RF_Capability
. . . . . . . fddRF_Capability
. . . . . . . tddRF_Capability
. . . . . . PhysicalChannelCapability
. . . . . . . fddPhysChCapability
. . . . . . . . DL_PhysChCapabilityFDD
. . . . . . . . . (IntegerType)maxNoDPCH_PDSCH_Codes[3] = 3
. . . . . . . . . (MaxNoPhysChBitsReceived)maxNoPhysChBitsReceived[4] = 6
. . . . . . . . . (BooleanType)supportForSF_512 = FALSE
. . . . . . . . . (BooleanType)supportOfPDSCH = FALSE
. . . . . . . . . SimultaneousSCCPCH_DPCH_Reception
. . . . . . . . UL_PhysChCapabilityFDD
. . . . . . . . . (MaxNoDPDCH_BitsTransmitted)maxNoDPDCH_BitsTransmitted[4] = 2
. . . . . . . . . (BooleanType)supportOfPCPCH = FALSE
. . . . . . . tddPhysChCapability
. . . . . . UE_MultiModeRAT_Capability
. . . . . . . MultiRAT_Capability
. . . . . . . . (BooleanType)supportOfGSM = FALSE
. . . . . . . . (BooleanType)supportOfMulticarrier = FALSE
. . . . . . . (MultiModeCapability)multiModeCapability[2] = 1
. . . . . . SecurityCapability
. . . . . . . (BitStringType)cipheringAlgorithmCap[16] = '0000000000000001'B
. . . . . . . (BitStringType)integrityProtectionAlgorithmCap[16] = '0000000000000010'B
. . . . . . UE_Positioning_Capability
. . . . . . . (BooleanType)standaloneLocMethodsSupported = FALSE
. . . . . . . (BooleanType)ue_BasedOTDOA_Supported = FALSE
. . . . . . . (NetworkAssistedGPS_Supported)networkAssistedGPS_Supported[2] = 1
. . . . . . . (BooleanType)supportForUE_GPS_TimingOfCellFrames = FALSE
. . . . . . . (BooleanType)supportForIPDL = FALSE
. . . . . . MeasurementCapability
. . . . . v370NonCriticalExtensions
. . . . . . RRCConnectionSetupComplete_v370ext
. . . . . . . UE_RadioAccessCapability_v370ext
. . . . . . . . UE_RadioAccessCapabBandFDDList
. . . . . . . . . UE_RadioAccessCapabBandFDD
. . . . . . . . . . (RadioFrequencyBandFDD)radioFrequencyBandFDD[3] = 1
. . . . . . . . . . fddRF_Capability
. . . . . . . . . . . (UE_PowerClassExt)ue_PowerClass[3] = 3
. . . . . . . . . . . (TxRxFrequencySeparation)txRxFrequencySeparation[2] = 0
. . . . . . . . . . MeasurementCapabilityExt
. . . . . . . . . . . CompressedModeMeasCapabFDDList
. . . . . . . . . . . . CompressedModeMeasCapabFDD
. . . . . . . . . . . . . (RadioFrequencyBandFDD)radioFrequencyBandFDD[3] = 1
. . . . . . . . . . . . . (BooleanType)dl_MeasurementsFDD = TRUE
. . . . . . . . . . . . . (BooleanType)ul_MeasurementsFDD = TRUE
. . . . . . . . . . . CompressedModeMeasCapabGSMList
. . . . . . . . . . . . CompressedModeMeasCapabGSM
. . . . . . . . . . . . . (RadioFrequencyBandGSM)radioFrequencyBandGSM[4] = 2
. . . . . . . . . . . . . (BooleanType)dl_MeasurementsGSM = FALSE
. . . . . . . . . . . . . (BooleanType)ul_MeasurementsGSM = FALSE
. . . . . . . . . . . . CompressedModeMeasCapabGSM
. . . . . . . . . . . . . (RadioFrequencyBandGSM)radioFrequencyBandGSM[4] = 6
. . . . . . . . . . . . . (BooleanType)dl_MeasurementsGSM = FALSE
. . . . . . . . . . . . . (BooleanType)ul_MeasurementsGSM = TRUE
. . . . . . . . . . . CompressedModeMeasCapabMC
. . . . . . v380NonCriticalExtensions
- Constraint:
car_RRC_ConnSetupCmpl
- BinaryMessage:
30 2a 02 01 ff 02 01 02 0a 05 01 00 00 00 00 4a 8b ff ff e0 00 04 91 a0 51 06 a4 c2 68 46 09 30 20 80 00 80 01 08 89 62 13 89 0c 80

- No.: 2054
- Timestamp: 17:23:39:537_1
- RFN: 78733
- Chip: 5376
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2072
- Timestamp: 17:23:39:664_0
- RFN: 78745
- Chip: 32000
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: tc_12_4_1_4c2:lt_LocUpateStep8 LINE 6
- Message Structure:
RRC_DataInd
. (IntegerType)cellId[0] = -1
. (SS_RB_Identity)rB_Id[0] = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain[0] = 0
. (START_Value)start[20] = '11111111111111111111'B
. LOCATIONUPDATINGREQUEST
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)mMProtocolDiscriminator[4] = '0101'B
. . (MsgType)msgType[8] = '00001000'B
. . CiphKeySeqNum
. . . (B1)spare1[1] = '0'B
. . . (KeySeq)keySeq[3] = '111'B
. . LocUpdType
. . . (B1)fOR[1] = '0'B
. . . (B1)spare1[1] = '0'B
. . . (B2)lUT[2] = '01'B
. . LocAreaId_v
. . . (OctetStringType)plmn[3] = '00F110'O
. . . (OctetStringType)lac[2] = '0001'O
. . MS_Clsmk1
. . . (B1)spare1[1] = '0'B
. . . (B2)revLvl[2] = '10'B
. . . (B1)eSIND[1] = '0'B
. . . (B1)a5_1[1] = '1'B
. . . (B3)rFPwrCap[3] = '111'B
. . MS_Identity_lv
. . . (Length)iel[1] = '08'O
. . . (B4)iDigit1[4] = '0000'B
. . . (B1)oddEvenInd[1] = '1'B
. . . (B3)typeOfId[3] = '001'B
. . . (OctetStringType)otherDigits[7] = '10101032547698'O
. . MS_Clsmk2
. . . (IEI8)iei[8] = '00110011'B
. . . (Length)iel[1] = '03'O
. . . (B1)spare1_1[1] = '0'B
. . . (B2)revLvl[2] = '10'B
. . . (B1)eSIND[1] = '0'B
. . . (B1)a5_1[1] = '1'B
. . . (B3)rFPwrCap[3] = '111'B
. . . (B1)spare1_2[1] = '0'B
. . . (B1)pSCap[1] = '0'B
. . . (B2)sSSI[2] = '01'B
. . . (B1)sMCap[1] = '1'B
. . . (B1)vBS[1] = '0'B
. . . (B1)vGCS[1] = '0'B
. . . (B1)fC[1] = '0'B
. . . (B1)cM3[1] = '1'B
. . . (B1)spare1_3[1] = '0'B
. . . (B1)lCSVA[1] = '0'B
. . . (B1)uCS2[1] = '0'B
. . . (B1)soLSA[1] = '0'B
. . . (B1)cMSP[1] = '0'B
. . . (B1)a5_3[1] = '0'B
. . . (B1)a5_2[1] = '0'B
- Constraint:
car_InitDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 00 03 04 04 ff ff f0 05 08 71 00 f1 10 00 01 4f 08 09 10 10 10 32 54 76 98 33 03 4f 18 80

- No.: 2108
- Timestamp: 17:23:39:670_0
- RFN: 78746
- Chip: 18176
- Event: Send
- PCO: Dc
- Message: RRC_DataReq
- Source: ts_MM_Authentication LINE 2
- Message Structure:
RRC_DataReq
. (IntegerType)cellId[-1] = -1
. (SS_RB_Identity)rB_Id[-1] = 3
. (LogicChGERAN)ch[-1] = -
. (SapId)sapId[1] = -
. (SS_CN_DomainIdentity)cN_Domain[-1] = 0
. AUTHENTICATIONREQUEST
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)mMProtocolDiscriminator[4] = '0101'B
. . (MsgType)msgType[8] = '00010010'B
. . (B4)spare4[4] = '0000'B
. . CiphKeySeqNum
. . . (B1)spare1[1] = '0'B
. . . (KeySeq)keySeq[3] = '000'B
. . (MM_RAND)rAND[128] = '01010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101'B
. . AUTN
. . . (IEI8)iei[8] = '00100000'B
. . . (Length)iel[1] = '10'O
. . . (BitStringType)aUTN[128] = '01100110000100010000000000110011001000101101110100000000000000000101010101000100011101110110011000010001000000000011001100100010'B
- Constraint:
ca_DataReq
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 00 05 12 00 55 55 55 55 55 55 55 55 55 55 55 55 55 55 55 55 20 10 66 11 00 33 22 dd 00 00 55 44 77 66 11 00 33 22

- No.: 2112
- Timestamp: 17:23:39:993_0
- RFN: 78778
- Chip: 28928
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_MM_Authentication LINE 3
- Message Structure:
RRC_DataInd
. (IntegerType)cellId[0] = -1
. (SS_RB_Identity)rB_Id[0] = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain[0] = 0
. (START_Value)start[0] = -
. AUTHENTICATIONRESPONSE
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)mMProtocolDiscriminator[4] = '0101'B
. . (MsgType)msgType[8] = '01010100'B
. . (AuthRsp)authRsp[32] = '01010101010001000111011101100110'B
. . AuthRspExt
. . . (IEI8)iei[8] = '00100001'B
. . . (Length)iel[1] = '04'O
. . . (BitStringType)rES[32] = '00010001000000000011001100100010'B
- Constraint:
car_UplinkDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 00 05 54 55 44 77 66 21 04 11 00 33 22

- No.: 2175
- Timestamp: 17:23:40:001_0
- RFN: 78779
- Chip: 22016
- Event: Send
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_REQ
- Source: ts_SS_DownloadSecurityKey:lt_DownloadKeyCRLC LINE 1
- Message Structure:
CRLC_SecurityMode_Config_REQ
. (IntegerType)cellId[-1] = -1
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity[0] = 0
. . (BitStringType)startValue[20] = "00000000000000000000"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = '01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100'B
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CRLC_SecurityModeCfgReq
- BinaryMessage:
30 21 02 01 ff 30 1c 0a 01 00 03 04 04 00 00 00 03 11 00 77 66 11 00 33 22 dd cc ff ee 99 88 bb aa 55 44

- No.: 2176
- Timestamp: 17:23:40:001_1
- RFN: 78779
- Chip: 23808
- Event: Receive
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_CNF
- Source: ts_SS_DownloadSecurityKey:lt_DownloadKeyCRLC LINE 2
- Message Structure:
CRLC_SecurityMode_Config_CNF
. (IntegerType)cellId[0] = -1
- Constraint:
ca_CRLC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 2183
- Timestamp: 17:23:40:002_5
- RFN: 78779
- Chip: 28416
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 1
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 0
. (IntegerType)count_I_LSB_UL[-1] = -
. (IntegerType)count_I_LSB_DL[-1] = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 00 02 01 00 02 01 00

- No.: 2184
- Timestamp: 17:23:40:003_0
- RFN: 78779
- Chip: 30208
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 2
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 0
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 00 02 01 00

- No.: 2185
- Timestamp: 17:23:40:003_1
- RFN: 78779
- Chip: 31744
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 3
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 1
. (IntegerType)count_I_LSB_UL[-1] = -
. (IntegerType)count_I_LSB_DL[-1] = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 01 02 01 00

- No.: 2186
- Timestamp: 17:23:40:004_0
- RFN: 78779
- Chip: 33280
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 4
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 1
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 2187
- Timestamp: 17:23:40:004_1
- RFN: 78779
- Chip: 35072
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 5
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 2
. (IntegerType)count_I_LSB_UL[-1] = -
. (IntegerType)count_I_LSB_DL[-1] = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 02 02 01 00

- No.: 2188
- Timestamp: 17:23:40:005_0
- RFN: 78779
- Chip: 36864
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 6
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 2
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 2189
- Timestamp: 17:23:40:005_1
- RFN: 78780
- Chip: 256
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 7
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 3
. (IntegerType)count_I_LSB_UL[-1] = -
. (IntegerType)count_I_LSB_DL[-1] = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 03 02 01 00

- No.: 2190
- Timestamp: 17:23:40:006_0
- RFN: 78780
- Chip: 1792
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 8
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 3
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 2191
- Timestamp: 17:23:40:006_1
- RFN: 78780
- Chip: 3584
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 9
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 4
. (IntegerType)count_I_LSB_UL[-1] = -
. (IntegerType)count_I_LSB_DL[-1] = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 04 02 01 00

- No.: 2192
- Timestamp: 17:23:40:006_2
- RFN: 78780
- Chip: 5120
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 10
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 4
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 2196
- Timestamp: 17:23:40:007_3
- RFN: 78780
- Chip: 8960
- Event: Send
- PCO: CRLC
- Message: CRLC_Integrity_Activate_REQ
- Source: ts_CRLC_DL_Integrity LINE 1
- Message Structure:
CRLC_Integrity_Activate_REQ
. (IntegerType)cellId[-1] = -1
. (CN_DomainIdentity)cn_DomainIdentity[0] = 0
. IntegrityActivationInfo
. . IntegrityProtectionModeInfo
. . . IntegrityProtectionModeCommand
. . . . startIntegrityProtection
. . . . . (BitStringType)integrityProtInitNumber[32] = "00000000000000000000000000000001"
. . . (IntegrityProtectionAlgorithm)integrityProtectionAlgorithm[0] = 0
- Constraint:
ca_CRLC_DL_IntegrityActivateReq
- BinaryMessage:
30 14 02 01 ff 0a 01 00 30 0c 30 07 03 05 00 00 00 00 01 0a 01 00

- No.: 2197
- Timestamp: 17:23:40:008_0
- RFN: 78780
- Chip: 11008
- Event: Receive
- PCO: CRLC
- Message: CRLC_Integrity_Activate_CNF
- Source: ts_CRLC_DL_Integrity LINE 2
- Message Structure:
CRLC_Integrity_Activate_CNF
. (IntegerType)cellId[0] = -1
- Constraint:
ca_CRLC_IntegrityActivateCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 2204
- Timestamp: 17:23:40:009_2
- RFN: 78780
- Chip: 15872
- Event: Send
- PCO: CRLC
- Message: CRLC_Integrity_Activate_REQ
- Source: ts_RB2_UL_IntegrityActivate LINE 1
- Message Structure:
CRLC_Integrity_Activate_REQ
. (IntegerType)cellId[-1] = -1
. (CN_DomainIdentity)cn_DomainIdentity[0] = 0
. IntegrityActivationInfo
. . IntegrityProtActivationInfoList
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity[-1] = 2
. . . . (IntegerType)rrc_MessageSequenceNumber[-1] = 0
- Constraint:
ca_CRLC_UL_IntegrityActivateReq
- BinaryMessage:
30 10 02 01 ff 0a 01 00 30 08 30 06 02 01 02 02 01 00

- No.: 2205
- Timestamp: 17:23:40:010_0
- RFN: 78780
- Chip: 17408
- Event: Receive
- PCO: CRLC
- Message: CRLC_Integrity_Activate_CNF
- Source: ts_RB2_UL_IntegrityActivate LINE 2
- Message Structure:
CRLC_Integrity_Activate_CNF
. (IntegerType)cellId[0] = -1
- Constraint:
ca_CRLC_IntegrityActivateCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 2212
- Timestamp: 17:23:40:011_0
- RFN: 78780
- Chip: 24064
- Event: Send
- PCO: AM
- Message: RLC_AM_DATA_REQ
- Source: ts_RRC_Security:lt_SendSecurityModeCommand LINE 8
- Message Structure:
RLC_AM_DATA_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 2
. AmConfirmationRequest
. aM_message
. . DL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00000000000000000000000000000000"
. . . . (IntegerType)rrc_MessageSequenceNumber[-1] = 0
. . . DL_DCCH_MessageType
. . . . SecurityModeCommand
. . . . . r3
. . . . . . SecurityModeCommand_r3_IEs
. . . . . . . (IntegerType)rrc_TransactionIdentifier[-1] = 0
. . . . . . . SecurityCapability
. . . . . . . . (BitStringType)cipheringAlgorithmCap[16] = '0000000000000001'B
. . . . . . . . (BitStringType)integrityProtectionAlgorithmCap[16] = '0000000000000010'B
. . . . . . . CipheringModeInfo
. . . . . . . IntegrityProtectionModeInfo
. . . . . . . . IntegrityProtectionModeCommand
. . . . . . . . . startIntegrityProtection
. . . . . . . . . . (BitStringType)integrityProtInitNumber[32] = "00000000000000000000000000000001"
. . . . . . . . (IntegrityProtectionAlgorithm)integrityProtectionAlgorithm[0] = 0
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity[0] = 0
. . . . . . . InterRAT_UE_SecurityCapList
. . . . . . . . InterRAT_UE_SecurityCapability
. . . . . . . . . gsm
. . . . . . . . . . (BitStringType)gsmSecurityCapability[7] = "0000000"
. . . . . . laterNonCriticalExtensions
- Constraint:
cas_RRC_SecModeCmd
- BinaryMessage:
30 18 02 01 ff 02 01 02 05 00 80 00 00 00 04 06 00 00 80 01 40 00 00 00 20 00

- No.: 2221
- Timestamp: 17:23:40:153_0
- RFN: 78794
- Chip: 30464
- Event: Receive
- PCO: AM
- Message: RLC_AM_DATA_IND
- Source: ts_RRC_Security:lt_StartSecurity_UE LINE 8
- Message Structure:
RLC_AM_DATA_IND
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 2
. IntegrityResult
. . (IntegrityStatus)integrityUsed[0] = 0
. aM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "01100100010100101000000110010100"
. . . . (IntegerType)rrc_MessageSequenceNumber[4] = 1
. . . UL_DCCH_MessageType
. . . . SecurityModeComplete
. . . . . (IntegerType)rrc_TransactionIdentifier[2] = 0
. . . . . IntegrityProtActivationInfo
. . . . . . RRC_MessageSequenceNumberList
. . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . (IntegerType)_elem[4] = 0
. . . . . laterNonCriticalExtensions
- Constraint:
car_RRC_SecModeCmpl
- BinaryMessage:
30 12 02 01 ff 02 01 02 0a 01 00 b2 29 40 ca 0d 21 00 00 00

- No.: 2222
- Timestamp: 17:23:40:154_0
- RFN: 78794
- Chip: 32000
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_Security:lt_StartSecurity_UE LINE 8
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2224
- Timestamp: 17:23:40:155_0
- RFN: 78794
- Chip: 35072
- Event: Send
- PCO: CRLC
- Message: CRLC_Integrity_Activate_REQ
- Source: ts_CRLC_UL_Integrity LINE 1
- Message Structure:
CRLC_Integrity_Activate_REQ
. (IntegerType)cellId[-1] = -1
. (CN_DomainIdentity)cn_DomainIdentity[0] = 0
. IntegrityActivationInfo
. . IntegrityProtActivationInfoList
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity[-1] = 0
. . . . (IntegerType)rrc_MessageSequenceNumber[-1] = 0
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity[-1] = 1
. . . . (IntegerType)rrc_MessageSequenceNumber[-1] = 0
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity[-1] = 3
. . . . (IntegerType)rrc_MessageSequenceNumber[-1] = 0
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity[-1] = 4
. . . . (IntegerType)rrc_MessageSequenceNumber[-1] = 0
- Constraint:
ca_CRLC_UL_IntegrityActivateReq
- BinaryMessage:
30 28 02 01 ff 0a 01 00 30 20 30 06 02 01 00 02 01 00 30 06 02 01 01 02 01 00 30 06 02 01 03 02 01 00 30 06 02 01 04 02 01 00

- No.: 2225
- Timestamp: 17:23:40:155_1
- RFN: 78794
- Chip: 37120
- Event: Receive
- PCO: CRLC
- Message: CRLC_Integrity_Activate_CNF
- Source: ts_CRLC_UL_Integrity LINE 2
- Message Structure:
CRLC_Integrity_Activate_CNF
. (IntegerType)cellId[0] = -1
- Constraint:
ca_CRLC_IntegrityActivateCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 2230
- Timestamp: 17:23:40:157_0
- RFN: 78795
- Chip: 4608
- Event: Send
- PCO: Dc
- Message: RRC_DataReq
- Source: tc_12_4_1_4c2:lt_LocUpateStep8 LINE 10
- Message Structure:
RRC_DataReq
. (IntegerType)cellId[-1] = -1
. (SS_RB_Identity)rB_Id[-1] = 3
. (LogicChGERAN)ch[-1] = -
. (SapId)sapId[1] = -
. (SS_CN_DomainIdentity)cN_Domain[-1] = 0
. LOCATIONUPDATINGACCEPT
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)mMProtocolDiscriminator[4] = '0101'B
. . (MsgType)msgType[8] = '00000010'B
. . LocAreaId_v
. . . (OctetStringType)plmn[3] = '00F110'O
. . . (OctetStringType)lac[2] = '0001'O
. . MM_MS_Identity
. . . (IEI8)iei[8] = '00010111'B
. . . (Length)iel[1] = '05'O
. . . (B4)iDigit1[4] = '1111'B
. . . (B1)oddEvenInd[1] = '0'B
. . . (B3)typeOfId[3] = '100'B
. . . (OctetStringType)otherDigits[-1] = '12345678'O
. . (FollowOnProceed)followOnProceed[8] = '10100001'B
. . (CTSPerm)cTSPerm[8] = '10100010'B
. . PLMN_List
- Constraint:
ca_DataReq
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 00 05 02 00 f1 10 00 01 17 05 f4 12 34 56 78 a1 a2

- No.: 2237
- Timestamp: 17:23:40:303_0
- RFN: 78809
- Chip: 30464
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: tc_12_4_1_4c2:lt_LocUpateStep8 LINE 11
- Message Structure:
RRC_DataInd
. (IntegerType)cellId[0] = -1
. (SS_RB_Identity)rB_Id[0] = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain[0] = 0
. (START_Value)start[0] = -
. TMSIREALLOCATIONCOMPLETE
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)mMProtocolDiscriminator[4] = '0101'B
. . (MsgType)msgType[8] = '10011011'B
- Constraint:
car_UplinkDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 00 05 9b

- No.: 2245
- Timestamp: 17:23:40:304_4
- RFN: 78809
- Chip: 34816
- Event: Start Timer
- Source: ts_RRC_Delay LINE 1
- Message Structure:
no details available
- Constraint:
t_Dly (1000 Ms)
- BinaryMessage:

- No.: 2249
- Timestamp: 17:23:41:304_0
- RFN: 78909
- Chip: 32256
- Event: Timeout
- Source: ts_RRC_Delay LINE 2
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 2254
- Timestamp: 17:23:41:305_2
- RFN: 78909
- Chip: 37376
- Event: Send
- PCO: UM
- Message: RLC_UM_DATA_REQ
- Source: ts_RRC_ConnRel:lt_Send_RRC_ConnectionRelease LINE 3
- Message Structure:
RLC_UM_DATA_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 1
. uM_message
. . DL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00000000000000000000000000000000"
. . . . (IntegerType)rrc_MessageSequenceNumber[-1] = 0
. . . DL_DCCH_MessageType
. . . . RRCConnectionRelease
. . . . . r3
. . . . . . RRCConnectionRelease_r3_IEs
. . . . . . . (IntegerType)rrc_TransactionIdentifier[-1] = 0
. . . . . . . (IntegerType)n_308[-1] = 1
. . . . . . . (ReleaseCause)releaseCause[0] = 0
. . . . . . . Rplmn_Information
. . . . . . laterNonCriticalExtensions
. (BooleanType)specialLI = FALSE
- Constraint:
cas_RRC_ConnRelDCCH
- BinaryMessage:
30 10 02 01 ff 02 01 01 80 00 00 00 03 c8 00 01 01 00

- No.: 2258
- Timestamp: 17:23:41:433_0
- RFN: 78922
- Chip: 28928
- Event: Receive
- PCO: UM
- Message: RLC_UM_DATA_IND
- Source: ts_RRC_ConnRel:lt_Send_RRC_ConnectionRelease LINE 4
- Message Structure:
RLC_UM_DATA_IND
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 1
. IntegrityResult
. uM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00100111010100110001100010101000"
. . . . (IntegerType)rrc_MessageSequenceNumber[4] = 1
. . . UL_DCCH_MessageType
. . . . RRCConnectionReleaseComplete
. . . . . (IntegerType)rrc_TransactionIdentifier[2] = 0
. . . . . FailureCauseWithProtErr
. . . . . laterNonCriticalExtensions
- Constraint:
car_RRC_ConnRelCmplUM
- BinaryMessage:
30 0e 02 01 ff 02 01 01 05 00 93 a9 8c 54 0c 40

- No.: 2259
- Timestamp: 17:23:41:433_1
- RFN: 78922
- Chip: 30208
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ConnRel:lt_Send_RRC_ConnectionRelease LINE 4
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2262
- Timestamp: 17:23:41:434_1
- RFN: 78922
- Chip: 32000
- Event: Start Timer
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 1
- Message Structure:
no details available
- Constraint:
t_Dly (5000 Ms)
- BinaryMessage:

- No.: 2266
- Timestamp: 17:23:41:592_0
- RFN: 78938
- Chip: 28928
- Event: Receive
- PCO: UM
- Message: RLC_UM_DATA_IND
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 4
- Message Structure:
RLC_UM_DATA_IND
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 1
. IntegrityResult
. uM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "01100001101000101010011110101100"
. . . . (IntegerType)rrc_MessageSequenceNumber[4] = 2
. . . UL_DCCH_MessageType
. . . . RRCConnectionReleaseComplete
. . . . . (IntegerType)rrc_TransactionIdentifier[2] = 0
. . . . . FailureCauseWithProtErr
. . . . . laterNonCriticalExtensions
- Constraint:
car_RRC_ConnRelCmplUM
- BinaryMessage:
30 0e 02 01 ff 02 01 01 05 00 b0 d1 53 d6 14 40

- No.: 2268
- Timestamp: 17:23:41:594_1
- RFN: 78938
- Chip: 30720
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 4
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2274
- Timestamp: 17:23:41:595_1
- RFN: 78938
- Chip: 35840
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 1
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 01 0a 01 00 05 00

- No.: 2278
- Timestamp: 17:23:41:601_0
- RFN: 78939
- Chip: 18432
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 2281
- Timestamp: 17:23:41:601_3
- RFN: 78939
- Chip: 21504
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 2
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 02 0a 01 00 05 00

- No.: 2285
- Timestamp: 17:23:41:605_0
- RFN: 78939
- Chip: 35840
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 2288
- Timestamp: 17:23:41:606_0
- RFN: 78940
- Chip: 512
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 3
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 03 0a 01 00 05 00

- No.: 2292
- Timestamp: 17:23:41:612_0
- RFN: 78940
- Chip: 25088
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 3
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 2295
- Timestamp: 17:23:41:613_2
- RFN: 78940
- Chip: 28160
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 4
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 04 0a 01 00 05 00

- No.: 2299
- Timestamp: 17:23:41:621_0
- RFN: 78941
- Chip: 18944
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 4
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 2302
- Timestamp: 17:23:41:622_0
- RFN: 78941
- Chip: 25088
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 1
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 136
. . . . . UL_RLC_Mode
. . . . . . UL_UM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (NoExplicitDiscard)timerBasedNoExplicit[0] = 9
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 1
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 1
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_UM_Info
- BinaryMessage:
30 22 02 01 ff 02 01 01 0a 01 00 30 17 30 0d 05 00 30 09 02 02 00 88 30 03 0a 01 09 30 06 02 01 01 02 01 01

- No.: 2306
- Timestamp: 17:23:41:630_0
- RFN: 78942
- Chip: 16640
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 2307
- Timestamp: 17:23:41:632_0
- RFN: 78942
- Chip: 23808
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 3
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 2
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 2
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 2
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 02 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 13 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 02 02 01 02

- No.: 2311
- Timestamp: 17:23:41:646_0
- RFN: 78944
- Chip: 512
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 4
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 2312
- Timestamp: 17:23:41:648_0
- RFN: 78944
- Chip: 7168
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 5
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 3
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 3
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 3
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 03 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 13 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 03 02 01 03

- No.: 2316
- Timestamp: 17:23:41:661_0
- RFN: 78945
- Chip: 20992
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 6
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 3
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 2317
- Timestamp: 17:23:41:663_0
- RFN: 78945
- Chip: 27648
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 7
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 4
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 4
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 4
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 04 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 13 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 04 02 01 04

- No.: 2321
- Timestamp: 17:23:41:675_0
- RFN: 78946
- Chip: 37376
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 8
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 4
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 2346
- Timestamp: 17:23:41:678_7
- RFN: 78947
- Chip: 11264
- Event: Start Timer
- Source: ts_NAS_Delay LINE 1
- Message Structure:
no details available
- Constraint:
t_Dly (5000 Ms)
- BinaryMessage:

- No.: 2353
- Timestamp: 17:23:46:684_0
- RFN: 79447
- Chip: 34816
- Event: Timeout
- Source: ts_NAS_Delay LINE 2
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 2360
- Timestamp: 17:23:46:685_4
- RFN: 79448
- Chip: 1280
- Event: Send
- PCO: Ut
- Message: MMI_CmdReq
- Source: ts_MMI_UE_SwitchOff LINE 2
- Message Structure:
MMI_CmdReq
. (IA5StringType)cmd[-1] = "Please switch off the UE"
- Constraint:
ca_MMI_CmdReq
- BinaryMessage:
50 6c 65 61 73 65 20 73 77 69 74 63 68 20 6f 66 66 20 20 74 68 65 20 55 45

- No.: 2364
- Timestamp: 17:23:48:053_0
- RFN: 79584
- Chip: 30976
- Event: Receive
- PCO: Ut
- Message: MMI_CmdCnf
- Source: ts_MMI_UE_SwitchOff LINE 3
- Message Structure:
MMI_CmdCnf
. (BooleanType)result = TRUE
. (IA5StringType)resultString[0] = ""
- Constraint:
ca_MMI_CmdCnf
- BinaryMessage:
80

- No.: 2383
- Timestamp: 17:23:48:055_3
- RFN: 79585
- Chip: 2048
- Event: Receive
- PCO: CPHY
- Message: CPHY_Out_of_Sync_IND
- Source: RRC_DefConnEst LINE 7
- Message Structure:
CPHY_Out_of_Sync_IND
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 20
- Constraint:
ca_OutOfSyncInd
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 2385
- Timestamp: 17:23:48:055_5
- RFN: 79585
- Chip: 3328
- Event: Default
- Source: RRC_DefConnEst LINE 0
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2386
- Timestamp: 17:23:48:056_0
- RFN: 79585
- Chip: 3840
- Event: Default
- Source: ts_RRC_ConnEst:lt_RcvConnReq LINE 4
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2391
- Timestamp: 17:23:55:150_0
- RFN: 80294
- Chip: 21504
- Event: Receive
- PCO: TM
- Message: RLC_TR_DATA_IND
- Source: ts_RRC_ConnEst:lt_RcvConnReq LINE 4
- Message Structure:
RLC_TR_DATA_IND
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 0
. tM_message
. . UL_CCCH_Message
. . . IntegrityCheckInfo
. . . UL_CCCH_MessageType
. . . . RRCConnectionRequest
. . . . . InitialUE_Identity
. . . . . . TMSI_and_LAI_GSM_MAP
. . . . . . . (BitStringType)tmsi[32] = "00010010001101000101011001111000"
. . . . . . . LAI
. . . . . . . . PLMN_Identity
. . . . . . . . . MCC
. . . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . . (IntegerType)_elem[4] = 1
. . . . . . . . . MNC
. . . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . . (IntegerType)_elem[4] = 1
. . . . . . . . (BitStringType)lac[16] = '0000000000000001'B
. . . . . (EstablishmentCause)establishmentCause[5] = 13
. . . . . (ProtocolErrorIndicator)protocolErrorIndicator[1] = 0
. . . . . MeasuredResultsOnRACH
. . . . . v3d0NonCriticalExtensions
- Constraint:
car_RRC_ConnReq
- BinaryMessage:
30 11 02 01 00 02 01 00 21 12 34 56 78 00 10 08 00 0b 40

- No.: 2395
- Timestamp: 17:23:55:160_0
- RFN: 80295
- Chip: 24064
- Event: Send
- PCO: UM
- Message: RLC_UM_DATA_REQ
- Source: ts_RRC_ConnEst:lt_Send_ConnSetUp LINE 22
- Message Structure:
RLC_UM_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 0
. uM_message
. . DL_CCCH_Message
. . . IntegrityCheckInfo
. . . DL_CCCH_MessageType
. . . . RRCConnectionSetup
. . . . . r3
. . . . . . RRCConnectionSetup_r3_IEs
. . . . . . . InitialUE_Identity
. . . . . . . . TMSI_and_LAI_GSM_MAP
. . . . . . . . . (BitStringType)tmsi[32] = "00010010001101000101011001111000"
. . . . . . . . . LAI
. . . . . . . . . . PLMN_Identity
. . . . . . . . . . . MCC
. . . . . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . . . . (IntegerType)_elem[4] = 1
. . . . . . . . . . . MNC
. . . . . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . . . . (IntegerType)_elem[4] = 1
. . . . . . . . . . (BitStringType)lac[16] = '0000000000000001'B
. . . . . . . (IntegerType)rrc_TransactionIdentifier[-1] = 0
. . . . . . . (IntegerType)activationTime[-1] = -
. . . . . . . U_RNTI
. . . . . . . . (BitStringType)srnc_Identity[12] = "000000000001"
. . . . . . . . (BitStringType)s_RNTI[20] = "00000000000000000001"
. . . . . . . (BitStringType)new_c_RNTI[16] = -
. . . . . . . (RRC_StateIndicator)rrc_StateIndicator[0] = 0
. . . . . . . (IntegerType)utran_DRX_CycleLengthCoeff[-1] = 9
. . . . . . . CapabilityUpdateRequirement
. . . . . . . . (BooleanType)ue_RadioCapabilityFDDUpdateRequirement = TRUE
. . . . . . . . (BooleanType)ue_RadioCapabilityTDDUpdateRequirement = FALSE
. . . . . . . . SystemSpecificCapUpdateReqList
. . . . . . . . . (SystemSpecificCapUpdateReq)_elem[0] = 0
. . . . . . . SRB_InformationSetupList2
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity[-1] = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_UM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 1
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex[-1] = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 1
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity[-1] = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 2
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 2
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 2
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 2
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex[-1] = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 2
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 2
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity[-1] = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 3
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 3
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 3
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 3
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex[-1] = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 3
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 3
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity[-1] = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 4
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 4
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 4
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 4
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex[-1] = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 4
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 4
. . . . . . . UL_CommonTransChInfo
. . . . . . . . TFC_Subset
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . TFCS
. . . . . . . . . . . ExplicitTFCS_Configuration
. . . . . . . . . . . . TFCS_ReconfAdd
. . . . . . . . . . . . . ctfcSize
. . . . . . . . . . . . . . ctfc2Bit
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . . . . . . . (IntegerType)ctfc2[-1] = 0
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . . . . . . . (IntegerType)ctfc2[-1] = 1
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC[-1] = 11
. . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaD[-1] = 15
. . . . . . . . . . . . . . . . . . . (IntegerType)referenceTFC_ID[-1] = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . UL_AddReconfTransChInfoList
. . . . . . . . UL_AddReconfTransChInformation
. . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType[0] = 0
. . . . . . . . . (IntegerType)transportChannelIdentity[-1] = 5
. . . . . . . . . TransportFormatSet
. . . . . . . . . . DedicatedTransChTFS
. . . . . . . . . . . tti
. . . . . . . . . . . . DedicatedDynamicTF_InfoList
. . . . . . . . . . . . . DedicatedDynamicTF_Info
. . . . . . . . . . . . . . rlc_Size
. . . . . . . . . . . . . . . BitModeRLC_SizeInfo
. . . . . . . . . . . . . . . . sizeType2
. . . . . . . . . . . . . . . . . (IntegerType)part1[-1] = 2
. . . . . . . . . . . . . . . . . (IntegerType)part2[-1] = -
. . . . . . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . LogicalChannelList
. . . . . . . . . . . SemistaticTF_Information
. . . . . . . . . . . . ChannelCodingType
. . . . . . . . . . . . . (CodingRate)convolutional[0] = 1
. . . . . . . . . . . . (IntegerType)rateMatchingAttribute[-1] = 192
. . . . . . . . . . . . (CRC_Size)crc_Size[0] = 3
. . . . . . . DL_CommonTransChInfo
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . dl_Parameters
. . . . . . . DL_AddReconfTransChInfoList
. . . . . . . . DL_AddReconfTransChInformation
. . . . . . . . . (DL_TrCH_Type)dl_TransportChannelType[0] = 0
. . . . . . . . . (IntegerType)dl_transportChannelIdentity[-1] = 10
. . . . . . . . . tfs_SignallingMode
. . . . . . . . . . UL_TransportChannelIdentity
. . . . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType[0] = 0
. . . . . . . . . . . (IntegerType)ul_TransportChannelIdentity[-1] = 5
. . . . . . . . . QualityTarget
. . . . . . . . . . (IntegerType)bler_QualityValue[-1] = -20
. . . . . . . . . TM_SignallingInfo
. . . . . . . FrequencyInfo
. . . . . . . (IntegerType)maxAllowedUL_TX_Power[-1] = -
. . . . . . . UL_ChannelRequirement
. . . . . . . . UL_DPCH_Info
. . . . . . . . . UL_DPCH_PowerControlInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (IntegerType)dpcch_PowerOffset[-1] = -40
. . . . . . . . . . . (IntegerType)pc_Preamble[-1] = 1
. . . . . . . . . . . (IntegerType)sRB_delay[-1] = 7
. . . . . . . . . . . PowerControlAlgorithm
. . . . . . . . . . . . (IntegerType)algorithm1[-1] = 1
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (ScramblingCodeType)scramblingCodeType[0] = 1
. . . . . . . . . . . (IntegerType)scramblingCode[-1] = 0
. . . . . . . . . . . (IntegerType)numberOfDPDCH[-1] = -
. . . . . . . . . . . (SpreadingFactor)spreadingFactor[0] = 4
. . . . . . . . . . . (BooleanType)tfci_Existence = TRUE
. . . . . . . . . . . (IntegerType)numberOfFBI_Bits[-1] = -
. . . . . . . . . . . (PuncturingLimit)puncturingLimit[0] = 15
. . . . . . . DL_CommonInformation
. . . . . . . . DL_DPCH_InfoCommon
. . . . . . . . . cfnHandling
. . . . . . . . . . initialise
. . . . . . . . . . . (IntegerType)cfntargetsfnframeoffset[-1] = -
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . DL_DPCH_PowerControlInfo
. . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . (DPC_Mode)dpc_Mode[0] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPilot_pdpdch[-1] = 0
. . . . . . . . . . . Dl_rate_matching_restriction
. . . . . . . . . . . SF512_AndPilot
. . . . . . . . . . . . (PilotBits128)sfd128[0] = 0
. . . . . . . . . . . (PositionFixedOrFlexible)positionFixedOrFlexible[0] = 0
. . . . . . . . . . . (BooleanType)tfci_Existence = FALSE
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . (IntegerType)defaultDPCH_OffsetValue[-1] = 459
. . . . . . . . . . DPCH_CompressedModeInfo
. . . . . . . . . . (TX_DiversityMode)tx_DiversityMode[0] = 0
. . . . . . . . . . SSDT_Information
. . . . . . . DL_InformationPerRL_List
. . . . . . . . DL_InformationPerRL
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . PrimaryCPICH_Info
. . . . . . . . . . . . (IntegerType)primaryScramblingCode[-1] = 100
. . . . . . . . . . . PDSCH_SHO_DCH_Info
. . . . . . . . . . . PDSCH_CodeMapping
. . . . . . . . . DL_DPCH_InfoPerRL
. . . . . . . . . . fdd
. . . . . . . . . . . (PCPICH_UsageForChannelEst)pCPICH_UsageForChannelEst[0] = 0
. . . . . . . . . . . (IntegerType)dpch_FrameOffset[-1] = 18
. . . . . . . . . . . SecondaryCPICH_Info
. . . . . . . . . . . DL_ChannelisationCodeList
. . . . . . . . . . . . DL_ChannelisationCode
. . . . . . . . . . . . . (IntegerType)secondaryScramblingCode[-1] = 1
. . . . . . . . . . . . . SF512_AndCodeNumber
. . . . . . . . . . . . . . (IntegerType)sf128[-1] = 0
. . . . . . . . . . . . . (ScramblingCodeChange)scramblingCodeChange[0] = 1
. . . . . . . . . . . (IntegerType)tpc_CombinationIndex[-1] = 0
. . . . . . . . . . . (SSDT_CellIdentity)ssdt_CellIdentity[0] = -
. . . . . . . . . . . (ClosedLoopTimingAdjMode)closedLoopTimingAdjMode[0] = -
. . . . . . . . . SCCPCH_InfoForFACH
. . . . . . laterNonCriticalExtensions
. (BooleanType)specialLI = TRUE
- Constraint:
cas_RRC_ConnSetup
- BinaryMessage:
30 78 02 01 00 02 01 00 30 e7 22 46 8a cf 00 02 01 00 01 00 04 00 00 4d 82 69 3a 10 10 89 0d 42 00 02 81 9e 8e 46 c9 a6 7c 9c 4e 74 20 a5 12 3a 8c 00 15 13 3d 1c 8d 93 4c f9 38 9c e8 42 52 24 b5 28 00 4a 46 7a 39 1b 26 99 f2 71 39 d0 86 b4 49 ea 70 00 d4 c8 00 06 25 2b f0 02 00 08 82 23 bf 66 08 98 95 a5 47 a2 00 00 01 3f 90 0a 14 e5 82 06 40 09 0c 28 08 01 01 ff

- No.: 2416
- Timestamp: 17:23:55:183_3
- RFN: 80297
- Chip: 34048
- Event: Start Timer
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 3
- Message Structure:
no details available
- Constraint:
t_WaitMS (13500 Ms)
- BinaryMessage:

- No.: 2423
- Timestamp: 17:23:55:402_1
- RFN: 80319
- Chip: 28928
- Event: Receive
- PCO: CPHY
- Message: CPHY_Sync_IND
- Source: RRC_DefConnEst LINE 5
- Message Structure:
CPHY_Sync_IND
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 20
- Constraint:
ca_SyncInd
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 2425
- Timestamp: 17:23:55:402_3
- RFN: 80319
- Chip: 30464
- Event: Default
- Source: RRC_DefConnEst LINE 0
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2426
- Timestamp: 17:23:55:403_0
- RFN: 80319
- Chip: 30976
- Event: Default
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2433
- Timestamp: 17:23:55:524_0
- RFN: 80331
- Chip: 37120
- Event: Receive
- PCO: AM
- Message: RLC_AM_DATA_IND
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
RLC_AM_DATA_IND
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 2
. IntegrityResult
. . (IntegrityStatus)integrityUsed[0] = 4294967296
. aM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . UL_DCCH_MessageType
. . . . RRCConnectionSetupComplete
. . . . . (IntegerType)rrc_TransactionIdentifier[2] = 0
. . . . . STARTList
. . . . . . STARTSingle
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity[1] = 0
. . . . . . . (BitStringType)start_Value[20] = "00000000000000000010"
. . . . . . STARTSingle
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity[1] = 1
. . . . . . . (BitStringType)start_Value[20] = "00000000000000000010"
. . . . . UE_RadioAccessCapability
. . . . . . (AccessStratumReleaseIndicator)accessStratumReleaseIndicator[0] = 0
. . . . . . PDCP_Capability
. . . . . . . (BooleanType)losslessSRNS_RelocationSupport = TRUE
. . . . . . . supportForRfc2507
. . . . . . RLC_Capability
. . . . . . . (TotalRLC_AM_BufferSize)totalRLC_AM_BufferSize[3] = 2
. . . . . . . (MaximumRLC_WindowSize)maximumRLC_WindowSize[1] = 0
. . . . . . . (MaximumAM_EntityNumberRLC_Cap)maximumAM_EntityNumber[3] = 3
. . . . . . TransportChannelCapability
. . . . . . . DL_TransChCapability
. . . . . . . . (MaxNoBits)maxNoBitsReceived[4] = 4
. . . . . . . . (MaxNoBits)maxConvCodeBitsReceived[4] = 0
. . . . . . . . TurboSupport
. . . . . . . . . (MaxNoBits)supported[4] = 4
. . . . . . . . (MaxSimultaneousTransChsDL)maxSimultaneousTransChs[2] = 1
. . . . . . . . (IntegerType)maxSimultaneousCCTrCH_Count[3] = 1
. . . . . . . . (MaxTransportBlocksDL)maxReceivedTransportBlocks[4] = 3
. . . . . . . . (MaxNumberOfTFC_DL)maxNumberOfTFC[4] = 5
. . . . . . . . (MaxNumberOfTF)maxNumberOfTF[3] = 1
. . . . . . . UL_TransChCapability
. . . . . . . . (MaxNoBits)maxNoBitsTransmitted[4] = 3
. . . . . . . . (MaxNoBits)maxConvCodeBitsTransmitted[4] = 0
. . . . . . . . TurboSupport
. . . . . . . . . (MaxNoBits)supported[4] = 3
. . . . . . . . (MaxSimultaneousTransChsUL)maxSimultaneousTransChs[3] = 2
. . . . . . . . modeSpecificInfo
. . . . . . . . (MaxTransportBlocksUL)maxTransmittedBlocks[4] = 2
. . . . . . . . (MaxNumberOfTFC_UL)maxNumberOfTFC[4] = 3
. . . . . . . . (MaxNumberOfTF)maxNumberOfTF[3] = 0
. . . . . . RF_Capability
. . . . . . . fddRF_Capability
. . . . . . . tddRF_Capability
. . . . . . PhysicalChannelCapability
. . . . . . . fddPhysChCapability
. . . . . . . . DL_PhysChCapabilityFDD
. . . . . . . . . (IntegerType)maxNoDPCH_PDSCH_Codes[3] = 3
. . . . . . . . . (MaxNoPhysChBitsReceived)maxNoPhysChBitsReceived[4] = 6
. . . . . . . . . (BooleanType)supportForSF_512 = FALSE
. . . . . . . . . (BooleanType)supportOfPDSCH = FALSE
. . . . . . . . . SimultaneousSCCPCH_DPCH_Reception
. . . . . . . . UL_PhysChCapabilityFDD
. . . . . . . . . (MaxNoDPDCH_BitsTransmitted)maxNoDPDCH_BitsTransmitted[4] = 2
. . . . . . . . . (BooleanType)supportOfPCPCH = FALSE
. . . . . . . tddPhysChCapability
. . . . . . UE_MultiModeRAT_Capability
. . . . . . . MultiRAT_Capability
. . . . . . . . (BooleanType)supportOfGSM = FALSE
. . . . . . . . (BooleanType)supportOfMulticarrier = FALSE
. . . . . . . (MultiModeCapability)multiModeCapability[2] = 1
. . . . . . SecurityCapability
. . . . . . . (BitStringType)cipheringAlgorithmCap[16] = '0000000000000001'B
. . . . . . . (BitStringType)integrityProtectionAlgorithmCap[16] = '0000000000000010'B
. . . . . . UE_Positioning_Capability
. . . . . . . (BooleanType)standaloneLocMethodsSupported = FALSE
. . . . . . . (BooleanType)ue_BasedOTDOA_Supported = FALSE
. . . . . . . (NetworkAssistedGPS_Supported)networkAssistedGPS_Supported[2] = 1
. . . . . . . (BooleanType)supportForUE_GPS_TimingOfCellFrames = FALSE
. . . . . . . (BooleanType)supportForIPDL = FALSE
. . . . . . MeasurementCapability
. . . . . v370NonCriticalExtensions
. . . . . . RRCConnectionSetupComplete_v370ext
. . . . . . . UE_RadioAccessCapability_v370ext
. . . . . . . . UE_RadioAccessCapabBandFDDList
. . . . . . . . . UE_RadioAccessCapabBandFDD
. . . . . . . . . . (RadioFrequencyBandFDD)radioFrequencyBandFDD[3] = 1
. . . . . . . . . . fddRF_Capability
. . . . . . . . . . . (UE_PowerClassExt)ue_PowerClass[3] = 3
. . . . . . . . . . . (TxRxFrequencySeparation)txRxFrequencySeparation[2] = 0
. . . . . . . . . . MeasurementCapabilityExt
. . . . . . . . . . . CompressedModeMeasCapabFDDList
. . . . . . . . . . . . CompressedModeMeasCapabFDD
. . . . . . . . . . . . . (RadioFrequencyBandFDD)radioFrequencyBandFDD[3] = 1
. . . . . . . . . . . . . (BooleanType)dl_MeasurementsFDD = TRUE
. . . . . . . . . . . . . (BooleanType)ul_MeasurementsFDD = TRUE
. . . . . . . . . . . CompressedModeMeasCapabGSMList
. . . . . . . . . . . . CompressedModeMeasCapabGSM
. . . . . . . . . . . . . (RadioFrequencyBandGSM)radioFrequencyBandGSM[4] = 2
. . . . . . . . . . . . . (BooleanType)dl_MeasurementsGSM = FALSE
. . . . . . . . . . . . . (BooleanType)ul_MeasurementsGSM = FALSE
. . . . . . . . . . . . CompressedModeMeasCapabGSM
. . . . . . . . . . . . . (RadioFrequencyBandGSM)radioFrequencyBandGSM[4] = 6
. . . . . . . . . . . . . (BooleanType)dl_MeasurementsGSM = FALSE
. . . . . . . . . . . . . (BooleanType)ul_MeasurementsGSM = TRUE
. . . . . . . . . . . CompressedModeMeasCapabMC
. . . . . . v380NonCriticalExtensions
- Constraint:
car_RRC_ConnSetupCmpl
- BinaryMessage:
30 2a 02 01 ff 02 01 02 0a 05 01 00 00 00 00 4a 88 00 00 a0 00 04 91 a0 51 06 a4 c2 68 46 09 30 20 80 00 80 01 08 89 62 13 89 0c 80

- No.: 2435
- Timestamp: 17:23:55:526_1
- RFN: 80332
- Chip: 6656
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2453
- Timestamp: 17:23:55:651_0
- RFN: 80344
- Chip: 29184
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_MM_IMSI_Detach:lt_IMSI_Detach LINE 2
- Message Structure:
RRC_DataInd
. (IntegerType)cellId[0] = -1
. (SS_RB_Identity)rB_Id[0] = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain[0] = 0
. (START_Value)start[20] = '00000000000000000010'B
. IMSIDETACHINDICATION
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)mMProtocolDiscriminator[4] = '0101'B
. . (MsgType)msgType[8] = '00000001'B
. . MS_Clsmk1
. . . (B1)spare1[1] = '0'B
. . . (B2)revLvl[2] = '10'B
. . . (B1)eSIND[1] = '0'B
. . . (B1)a5_1[1] = '1'B
. . . (B3)rFPwrCap[3] = '111'B
. . MS_Identity_lv
. . . (Length)iel[1] = '05'O
. . . (B4)iDigit1[4] = '1111'B
. . . (B1)oddEvenInd[1] = '0'B
. . . (B3)typeOfId[3] = '100'B
. . . (OctetStringType)otherDigits[4] = '12345678'O
- Constraint:
car_InitDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 00 03 04 04 00 00 20 05 01 4f 05 f4 12 34 56 78

- No.: 2454
- Timestamp: 17:23:55:652_0
- RFN: 80344
- Chip: 30720
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_MM_IMSI_Detach:lt_IMSI_Detach LINE 2
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2466
- Timestamp: 17:23:55:653_5
- RFN: 80344
- Chip: 36352
- Event: Start Timer
- Source: ts_RRC_Delay LINE 1
- Message Structure:
no details available
- Constraint:
t_Dly (1000 Ms)
- BinaryMessage:

- No.: 2470
- Timestamp: 17:23:56:646_0
- RFN: 80444
- Chip: 6912
- Event: Timeout
- Source: ts_RRC_Delay LINE 2
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 2475
- Timestamp: 17:23:56:647_2
- RFN: 80444
- Chip: 11520
- Event: Send
- PCO: UM
- Message: RLC_UM_DATA_REQ
- Source: ts_RRC_ConnRel:lt_Send_RRC_ConnectionRelease LINE 3
- Message Structure:
RLC_UM_DATA_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 1
. uM_message
. . DL_DCCH_Message
. . . IntegrityCheckInfo
. . . DL_DCCH_MessageType
. . . . RRCConnectionRelease
. . . . . r3
. . . . . . RRCConnectionRelease_r3_IEs
. . . . . . . (IntegerType)rrc_TransactionIdentifier[-1] = 0
. . . . . . . (IntegerType)n_308[-1] = 1
. . . . . . . (ReleaseCause)releaseCause[0] = 0
. . . . . . . Rplmn_Information
. . . . . . laterNonCriticalExtensions
. (BooleanType)specialLI = FALSE
- Constraint:
cas_RRC_ConnRelDCCH
- BinaryMessage:
30 0c 02 01 ff 02 01 01 3c 80 00 01 01 00

- No.: 2479
- Timestamp: 17:23:56:771_0
- RFN: 80456
- Chip: 28160
- Event: Receive
- PCO: UM
- Message: RLC_UM_DATA_IND
- Source: ts_RRC_ConnRel:lt_Send_RRC_ConnectionRelease LINE 4
- Message Structure:
RLC_UM_DATA_IND
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 1
. IntegrityResult
. uM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . UL_DCCH_MessageType
. . . . RRCConnectionReleaseComplete
. . . . . (IntegerType)rrc_TransactionIdentifier[2] = 0
. . . . . FailureCauseWithProtErr
. . . . . laterNonCriticalExtensions
- Constraint:
car_RRC_ConnRelCmplUM
- BinaryMessage:
30 0a 02 01 ff 02 01 01 05 00 44 00

- No.: 2480
- Timestamp: 17:23:56:772_0
- RFN: 80456
- Chip: 29440
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ConnRel:lt_Send_RRC_ConnectionRelease LINE 4
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2483
- Timestamp: 17:23:56:772_3
- RFN: 80456
- Chip: 31488
- Event: Start Timer
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 1
- Message Structure:
no details available
- Constraint:
t_Dly (5000 Ms)
- BinaryMessage:

- No.: 2487
- Timestamp: 17:23:56:931_0
- RFN: 80472
- Chip: 28672
- Event: Receive
- PCO: UM
- Message: RLC_UM_DATA_IND
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 4
- Message Structure:
RLC_UM_DATA_IND
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 1
. IntegrityResult
. uM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . UL_DCCH_MessageType
. . . . RRCConnectionReleaseComplete
. . . . . (IntegerType)rrc_TransactionIdentifier[2] = 0
. . . . . FailureCauseWithProtErr
. . . . . laterNonCriticalExtensions
- Constraint:
car_RRC_ConnRelCmplUM
- BinaryMessage:
30 0a 02 01 ff 02 01 01 05 00 44 00

- No.: 2489
- Timestamp: 17:23:56:931_2
- RFN: 80472
- Chip: 30208
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 4
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2495
- Timestamp: 17:23:56:933_0
- RFN: 80472
- Chip: 34816
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 1
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 01 0a 01 00 05 00

- No.: 2499
- Timestamp: 17:23:56:939_0
- RFN: 80473
- Chip: 20480
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 2502
- Timestamp: 17:23:56:940_0
- RFN: 80473
- Chip: 24064
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 2
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 02 0a 01 00 05 00

- No.: 2506
- Timestamp: 17:23:56:943_0
- RFN: 80473
- Chip: 36352
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 2509
- Timestamp: 17:23:56:944_0
- RFN: 80474
- Chip: 1024
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 3
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 03 0a 01 00 05 00

- No.: 2513
- Timestamp: 17:23:56:950_0
- RFN: 80474
- Chip: 25344
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 3
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 2516
- Timestamp: 17:23:56:951_0
- RFN: 80474
- Chip: 28928
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 4
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 04 0a 01 00 05 00

- No.: 2520
- Timestamp: 17:23:56:959_0
- RFN: 80475
- Chip: 18176
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 4
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 2523
- Timestamp: 17:23:56:961_0
- RFN: 80475
- Chip: 24576
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 1
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 136
. . . . . UL_RLC_Mode
. . . . . . UL_UM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (NoExplicitDiscard)timerBasedNoExplicit[0] = 9
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 1
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 1
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_UM_Info
- BinaryMessage:
30 22 02 01 ff 02 01 01 0a 01 00 30 17 30 0d 05 00 30 09 02 02 00 88 30 03 0a 01 09 30 06 02 01 01 02 01 01

- No.: 2527
- Timestamp: 17:23:56:970_0
- RFN: 80476
- Chip: 19968
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 2528
- Timestamp: 17:23:56:971_0
- RFN: 80476
- Chip: 26880
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 3
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 2
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 2
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 2
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 02 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 13 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 02 02 01 02

- No.: 2532
- Timestamp: 17:23:56:984_0
- RFN: 80477
- Chip: 36352
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 4
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 2533
- Timestamp: 17:23:56:985_0
- RFN: 80478
- Chip: 4352
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 5
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 3
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 3
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 3
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 03 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 13 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 03 02 01 03

- No.: 2537
- Timestamp: 17:23:57:000_0
- RFN: 80479
- Chip: 21760
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 6
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 3
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 2538
- Timestamp: 17:23:57:002_0
- RFN: 80479
- Chip: 28416
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 7
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 4
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 4
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 4
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 04 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 13 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 04 02 01 04

- No.: 2542
- Timestamp: 17:23:57:015_0
- RFN: 80481
- Chip: 3584
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 8
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 4
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 2565
- Timestamp: 17:23:57:018_4
- RFN: 80481
- Chip: 14848
- Event: Start Timer
- Source: ts_RRC_ConnRejectGMM_Detach LINE 1
- Message Structure:
no details available
- Constraint:
t_Dly (2000 Ms)
- BinaryMessage:

- No.: 2570
- Timestamp: 17:23:57:070_1
- RFN: 80486
- Chip: 24832
- Event: Receive
- PCO: CPHY
- Message: CPHY_Out_of_Sync_IND
- Source: RRC_DefConnEst LINE 7
- Message Structure:
CPHY_Out_of_Sync_IND
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 20
- Constraint:
ca_OutOfSyncInd
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 2572
- Timestamp: 17:23:57:071_1
- RFN: 80486
- Chip: 26368
- Event: Default
- Source: RRC_DefConnEst LINE 0
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2573
- Timestamp: 17:23:57:071_2
- RFN: 80486
- Chip: 26880
- Event: Default
- Source: ts_RRC_ConnRejectGMM_Detach LINE 4
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2578
- Timestamp: 17:23:59:020_0
- RFN: 80681
- Chip: 25344
- Event: Timeout
- Source: ts_RRC_ConnRejectGMM_Detach LINE 4
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 2614
- Timestamp: 17:23:59:025_0
- RFN: 80682
- Chip: 5888
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 1
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 01 0a 01 00 05 00

- No.: 2618
- Timestamp: 17:23:59:029_0
- RFN: 80682
- Chip: 20992
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 2621
- Timestamp: 17:23:59:030_0
- RFN: 80682
- Chip: 25344
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 2
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 02 0a 01 00 05 00

- No.: 2625
- Timestamp: 17:23:59:033_0
- RFN: 80682
- Chip: 37376
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 2628
- Timestamp: 17:23:59:034_1
- RFN: 80683
- Chip: 2304
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 3
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 03 0a 01 00 05 00

- No.: 2632
- Timestamp: 17:23:59:040_0
- RFN: 80683
- Chip: 25088
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 3
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 2635
- Timestamp: 17:23:59:041_0
- RFN: 80683
- Chip: 28416
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 4
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 04 0a 01 00 05 00

- No.: 2639
- Timestamp: 17:23:59:047_0
- RFN: 80684
- Chip: 14336
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 4
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 2643
- Timestamp: 17:23:59:048_2
- RFN: 80684
- Chip: 18688
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_CMAC_Rel LINE 1
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 26
. (RatType)ratType[0] = 0
. configMessage
- Constraint:
cas_MAC_Rel
- BinaryMessage:
30 0b 02 01 ff 02 01 1a 0a 01 00 05 00

- No.: 2647
- Timestamp: 17:23:59:051_0
- RFN: 80684
- Chip: 29440
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_CMAC_Rel LINE 2
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 26
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 1a

- No.: 2650
- Timestamp: 17:23:59:052_1
- RFN: 80684
- Chip: 33536
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_CMAC_Rel LINE 1
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 20
. (RatType)ratType[0] = 0
. configMessage
- Constraint:
cas_MAC_Rel
- BinaryMessage:
30 0b 02 01 ff 02 01 14 0a 01 00 05 00

- No.: 2654
- Timestamp: 17:23:59:057_0
- RFN: 80685
- Chip: 12288
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_CMAC_Rel LINE 2
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 20
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 14

- No.: 2657
- Timestamp: 17:23:59:057_3
- RFN: 80685
- Chip: 15104
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Release_REQ
- Source: ts_CPHY_TrChRelDCH_NoSHO LINE 1
- Message Structure:
CPHY_TrCH_Release_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 26
. TrChConfigType
. . (TrChConfigType_list_0)dch[0] = 0
- Constraint:
ca_PHY_RelReqDCH_NoSHO
- BinaryMessage:
30 09 02 01 00 02 01 1a 0a 01 00

- No.: 2661
- Timestamp: 17:23:59:062_0
- RFN: 80685
- Chip: 33792
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Release_CNF
- Source: ts_CPHY_TrChRelDCH_NoSHO LINE 2
- Message Structure:
CPHY_TrCH_Release_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 26
- Constraint:
ca_PHY_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 1a

- No.: 2664
- Timestamp: 17:23:59:063_1
- RFN: 80685
- Chip: 36864
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Release_REQ
- Source: ts_CPHY_TrChRelDCH_NoSHO LINE 1
- Message Structure:
CPHY_TrCH_Release_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 20
. TrChConfigType
. . (TrChConfigType_list_0)dch[0] = 0
- Constraint:
ca_PHY_RelReqDCH_NoSHO
- BinaryMessage:
30 09 02 01 00 02 01 14 0a 01 00

- No.: 2668
- Timestamp: 17:23:59:089_0
- RFN: 80688
- Chip: 22016
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Release_CNF
- Source: ts_CPHY_TrChRelDCH_NoSHO LINE 2
- Message Structure:
CPHY_TrCH_Release_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 20
- Constraint:
ca_PHY_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 2671
- Timestamp: 17:23:59:090_0
- RFN: 80688
- Chip: 24832
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 26
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 1a

- No.: 2675
- Timestamp: 17:23:59:098_0
- RFN: 80689
- Chip: 17408
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 26
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 1a

- No.: 2678
- Timestamp: 17:23:59:099_0
- RFN: 80689
- Chip: 20480
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 20
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 2682
- Timestamp: 17:23:59:122_0
- RFN: 80691
- Chip: 33792
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 20
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 2687
- Timestamp: 17:23:59:123_2
- RFN: 80691
- Chip: 37632
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 0
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 00 02 01 00 0a 01 00 05 00

- No.: 2691
- Timestamp: 17:23:59:127_0
- RFN: 80692
- Chip: 15872
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 0
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 00

- No.: 2694
- Timestamp: 17:23:59:128_2
- RFN: 80692
- Chip: 19712
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_CMAC_Rel LINE 1
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 8
. (RatType)ratType[0] = 0
. configMessage
- Constraint:
cas_MAC_Rel
- BinaryMessage:
30 0b 02 01 00 02 01 08 0a 01 00 05 00

- No.: 2698
- Timestamp: 17:23:59:130_0
- RFN: 80692
- Chip: 27648
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_CMAC_Rel LINE 2
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 8
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 08

- No.: 2701
- Timestamp: 17:23:59:131_2
- RFN: 80692
- Chip: 30720
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Release_REQ
- Source: ts_CPHY_TrChRelNonDch LINE 1
- Message Structure:
CPHY_TrCH_Release_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 8
. TrChConfigType
- Constraint:
ca_PHY_RelReqNonDch
- BinaryMessage:
30 08 02 01 00 02 01 08 05 00

- No.: 2705
- Timestamp: 17:23:59:164_0
- RFN: 80695
- Chip: 36608
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Release_CNF
- Source: ts_CPHY_TrChRelNonDch LINE 2
- Message Structure:
CPHY_TrCH_Release_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 8
- Constraint:
ca_PHY_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 08

- No.: 2708
- Timestamp: 17:23:59:164_3
- RFN: 80696
- Chip: 1280
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 7
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 07

- No.: 2712
- Timestamp: 17:23:59:169_0
- RFN: 80696
- Chip: 19200
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 7
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 07

- No.: 2715
- Timestamp: 17:23:59:170_0
- RFN: 80696
- Chip: 22016
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 8
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 08

- No.: 2719
- Timestamp: 17:23:59:224_0
- RFN: 80702
- Chip: 1280
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 8
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 08

- No.: 2722
- Timestamp: 17:23:59:225_2
- RFN: 80702
- Chip: 5120
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -2
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 00 02 01 fe 0a 01 00 05 00

- No.: 2726
- Timestamp: 17:23:59:228_0
- RFN: 80702
- Chip: 14336
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 fe

- No.: 2729
- Timestamp: 17:23:59:228_3
- RFN: 80702
- Chip: 17664
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_CMAC_Rel LINE 1
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 5
. (RatType)ratType[0] = 0
. configMessage
- Constraint:
cas_MAC_Rel
- BinaryMessage:
30 0b 02 01 00 02 01 05 0a 01 00 05 00

- No.: 2733
- Timestamp: 17:23:59:231_0
- RFN: 80702
- Chip: 28928
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_CMAC_Rel LINE 2
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 5
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 05

- No.: 2736
- Timestamp: 17:23:59:232_2
- RFN: 80702
- Chip: 31744
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Release_REQ
- Source: ts_CPHY_TrChRelNonDch LINE 1
- Message Structure:
CPHY_TrCH_Release_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 5
. TrChConfigType
- Constraint:
ca_PHY_RelReqNonDch
- BinaryMessage:
30 08 02 01 00 02 01 05 05 00

- No.: 2740
- Timestamp: 17:23:59:237_0
- RFN: 80703
- Chip: 13312
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Release_CNF
- Source: ts_CPHY_TrChRelNonDch LINE 2
- Message Structure:
CPHY_TrCH_Release_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 5
- Constraint:
ca_PHY_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 05

- No.: 2743
- Timestamp: 17:23:59:238_2
- RFN: 80703
- Chip: 16384
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 6
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 06

- No.: 2747
- Timestamp: 17:23:59:242_0
- RFN: 80703
- Chip: 29696
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 6
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 06

- No.: 2750
- Timestamp: 17:23:59:242_3
- RFN: 80703
- Chip: 32256
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 5
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 05

- No.: 2754
- Timestamp: 17:23:59:248_0
- RFN: 80704
- Chip: 14592
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 5
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 05

- No.: 2759
- Timestamp: 17:23:59:249_0
- RFN: 80704
- Chip: 18688
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 00 02 01 ff 0a 01 00 05 00

- No.: 2763
- Timestamp: 17:23:59:251_0
- RFN: 80704
- Chip: 28672
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 2766
- Timestamp: 17:23:59:252_2
- RFN: 80704
- Chip: 32256
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_CMAC_Rel LINE 1
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 4
. (RatType)ratType[0] = 0
. configMessage
- Constraint:
cas_MAC_Rel
- BinaryMessage:
30 0b 02 01 00 02 01 04 0a 01 00 05 00

- No.: 2770
- Timestamp: 17:23:59:256_0
- RFN: 80705
- Chip: 6912
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_CMAC_Rel LINE 2
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 4
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 04

- No.: 2773
- Timestamp: 17:23:59:256_3
- RFN: 80705
- Chip: 9728
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Release_REQ
- Source: ts_CPHY_TrChRelNonDch LINE 1
- Message Structure:
CPHY_TrCH_Release_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 4
. TrChConfigType
- Constraint:
ca_PHY_RelReqNonDch
- BinaryMessage:
30 08 02 01 00 02 01 04 05 00

- No.: 2777
- Timestamp: 17:23:59:261_0
- RFN: 80705
- Chip: 26368
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Release_CNF
- Source: ts_CPHY_TrChRelNonDch LINE 2
- Message Structure:
CPHY_TrCH_Release_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 4
- Constraint:
ca_PHY_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 04

- No.: 2780
- Timestamp: 17:23:59:261_3
- RFN: 80705
- Chip: 29440
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 2
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 02

- No.: 2784
- Timestamp: 17:23:59:265_0
- RFN: 80706
- Chip: 4352
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 2
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 02

- No.: 2787
- Timestamp: 17:23:59:266_0
- RFN: 80706
- Chip: 7168
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 1
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 01

- No.: 2791
- Timestamp: 17:23:59:269_0
- RFN: 80706
- Chip: 21504
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 1
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 01

- No.: 2794
- Timestamp: 17:23:59:270_2
- RFN: 80706
- Chip: 24064
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 4
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 04

- No.: 2798
- Timestamp: 17:23:59:275_0
- RFN: 80707
- Chip: 5632
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 4
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 04

- No.: 2801
- Timestamp: 17:23:59:276_1
- RFN: 80707
- Chip: 8192
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 0
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 00

- No.: 2805
- Timestamp: 17:23:59:280_0
- RFN: 80707
- Chip: 22528
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 0
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 00

- No.: 2872
- Timestamp: 17:23:59:289_1
- RFN: 80708
- Chip: 18944
- Event: Log
- PCO: VERDICT
- Message: PASS
- Source: tc_12_4_1_4c2 LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage: