**3GPP TSG-RAN WG2 Meeting #105R2-190xxxx**

**Athens, Greece, February 25th-March 1st 2019**

|  |
| --- |
| *CR-Form-v11.4* |
| **CHANGE REQUEST** |
|  |
|  | **36.331** | **CR** | **3868** | **rev** | **2** | **Current version:** | **15.4.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network | **X** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Clarification on timing reference cell of smtc configuration |
|  |  |
| ***Source to WG:*** | MediaTek Inc. |
| ***Source to TSG:*** | R2 |
|  |  |
| ***Work item code:*** | NR\_newRAT-Core |  | ***Date:*** | 02/25/2019 |
|  |  |  |  |  |
| ***Category:*** | F |  | ***Release:*** | Rel-15 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)**Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)* |
|  |  |
| ***Reason for change:*** | In RAN2#103 meeting, RAN2 agreed to add SMTC configuration for NR mobility procedure (R2-1813261). And in 38.331, CR 270 (R2-1817861) is agreed to clarify the timing reference cell in SMTC configuration. We think similar clarification should also be applied in LTE. In case LTE handover is triggered with SN Change or NR PSCell addition procedure, it is unclear whether the timing reference cell is source PCell or target PCell. As the handover command is generated by the target cell, we think it is more reasonable to use target PCell as timing reference cell.  |
|  |  |
| ***Summary of change:*** | Indicate that the *smtc* in *RRCConnectionReconfiguration* refers to the **target** PCell.**Impact analysis**Impacted 5G architecture options: EN-DCImpacted functionality: NR mobility procedure including NR PSCell addition and SN change in EN-DCInter-operability:if the UE implements the CR but the network does not or vice-versa, the UE and NW may have different understanding on the timing reference cell for the SMTC configuration. The consequences if not approved remain. |
|  |  |
| ***Consequences if not approved:*** | The UE and the NW may have different understanding on the timing reference cell in case LTE handover is triggered with NR PSCell addition or SN Change. The UE may fail to find the NR target cell and result in NR mobility procedure failed.  |
|  |  |
| ***Clauses affected:*** | 6.2.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **x** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **x** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **x** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |

### 6.2.2 Message definitions

<Skip unrelated Parts>

#### – *RRCConnectionReconfiguration*

The *RRCConnectionReconfiguration* message is the command to modify an RRC connection. It may convey information for measurement configuration, mobility control, radio resource configuration (including RBs, MAC main configuration and physical channel configuration) including any associated dedicated NAS information and security configuration.

Signalling radio bearer: SRB1

RLC-SAP: AM

Logical channel: DCCH

Direction: E‑UTRAN to UE

*RRCConnectionReconfiguration message*

-- ASN1START

RRCConnectionReconfiguration ::= SEQUENCE {

 rrc-TransactionIdentifier RRC-TransactionIdentifier,

 criticalExtensions CHOICE {

 c1 CHOICE{

 rrcConnectionReconfiguration-r8 RRCConnectionReconfiguration-r8-IEs,

 spare7 NULL,

 spare6 NULL, spare5 NULL, spare4 NULL,

 spare3 NULL, spare2 NULL, spare1 NULL

 },

 criticalExtensionsFuture SEQUENCE {}

 }

}

RRCConnectionReconfiguration-r8-IEs ::= SEQUENCE {

 measConfig MeasConfig OPTIONAL, -- Need ON

 mobilityControlInfo MobilityControlInfo OPTIONAL, -- Cond HO

 dedicatedInfoNASList SEQUENCE (SIZE(1..maxDRB)) OF

 DedicatedInfoNAS OPTIONAL, -- Cond nonHO

 radioResourceConfigDedicated RadioResourceConfigDedicated OPTIONAL, -- Cond HO-toEUTRA

 securityConfigHO SecurityConfigHO OPTIONAL, -- Cond HO-toEPC

 nonCriticalExtension RRCConnectionReconfiguration-v890-IEs OPTIONAL

}

RRCConnectionReconfiguration-v890-IEs ::= SEQUENCE {

 lateNonCriticalExtension OCTET STRING (CONTAINING RRCConnectionReconfiguration-v8m0-IEs) OPTIONAL,

 nonCriticalExtension RRCConnectionReconfiguration-v920-IEs OPTIONAL

}

-- Late non-critical extensions:

RRCConnectionReconfiguration-v8m0-IEs ::= SEQUENCE {

 -- Following field is only for pre REL-10 late non-critical extensions

 lateNonCriticalExtension OCTET STRING OPTIONAL,

 nonCriticalExtension RRCConnectionReconfiguration-v10i0-IEs OPTIONAL

}

RRCConnectionReconfiguration-v10i0-IEs ::= SEQUENCE {

 antennaInfoDedicatedPCell-v10i0 AntennaInfoDedicated-v10i0 OPTIONAL, -- Need ON

 nonCriticalExtension RRCConnectionReconfiguration-v10l0-IEs OPTIONAL

}

RRCConnectionReconfiguration-v10l0-IEs ::= SEQUENCE {

 mobilityControlInfo-v10l0 MobilityControlInfo-v10l0 OPTIONAL,

 sCellToAddModList-v10l0 SCellToAddModList-v10l0 OPTIONAL, -- Need ON

 -- Following field is only for late non-critical extensions from REL-10 to REL-11

 lateNonCriticalExtension OCTET STRING OPTIONAL,

 nonCriticalExtension RRCConnectionReconfiguration-v12f0-IEs OPTIONAL

}

RRCConnectionReconfiguration-v12f0-IEs ::= SEQUENCE {

 scg-Configuration-v12f0 SCG-Configuration-v12f0 OPTIONAL, -- Cond nonFullConfig

 -- Following field is only for late non-critical extensions from REL-12

 lateNonCriticalExtension OCTET STRING OPTIONAL,

 nonCriticalExtension RRCConnectionReconfiguration-v1370-IEs OPTIONAL

}

RRCConnectionReconfiguration-v1370-IEs ::= SEQUENCE {

 radioResourceConfigDedicated-v1370 RadioResourceConfigDedicated-v1370 OPTIONAL, -- Need ON

 sCellToAddModListExt-v1370 SCellToAddModListExt-v1370 OPTIONAL, -- Need ON

 nonCriticalExtension RRCConnectionReconfiguration-v13c0-IEs OPTIONAL

}

RRCConnectionReconfiguration-v13c0-IEs ::= SEQUENCE {

 radioResourceConfigDedicated-v13c0 RadioResourceConfigDedicated-v13c0 OPTIONAL, -- Need ON

 sCellToAddModList-v13c0 SCellToAddModList-v13c0 OPTIONAL, -- Need ON

 sCellToAddModListExt-v13c0 SCellToAddModListExt-v13c0 OPTIONAL, -- Need ON

 scg-Configuration-v13c0 SCG-Configuration-v13c0 OPTIONAL, -- Need ON

 -- Following field is only for late non-critical extensions from REL-13 onwards

 nonCriticalExtension SEQUENCE {} OPTIONAL

}

-- Regular non-critical extensions:

RRCConnectionReconfiguration-v920-IEs ::= SEQUENCE {

 otherConfig-r9 OtherConfig-r9 OPTIONAL, -- Need ON

 fullConfig-r9 ENUMERATED {true} OPTIONAL, -- Cond HO-Reestab

 nonCriticalExtension RRCConnectionReconfiguration-v1020-IEs OPTIONAL

}

RRCConnectionReconfiguration-v1020-IEs ::= SEQUENCE {

 sCellToReleaseList-r10 SCellToReleaseList-r10 OPTIONAL, -- Need ON

 sCellToAddModList-r10 SCellToAddModList-r10 OPTIONAL, -- Need ON

 nonCriticalExtension RRCConnectionReconfiguration-v1130-IEs OPTIONAL

}

RRCConnectionReconfiguration-v1130-IEs ::= SEQUENCE {

 systemInformationBlockType1Dedicated-r11 OCTET STRING (CONTAINING SystemInformationBlockType1) OPTIONAL, -- Need ON

 nonCriticalExtension RRCConnectionReconfiguration-v1250-IEs OPTIONAL

}

RRCConnectionReconfiguration-v1250-IEs ::= SEQUENCE {

 wlan-OffloadInfo-r12 CHOICE {

 release NULL,

 setup SEQUENCE {

 wlan-OffloadConfigDedicated-r12 WLAN-OffloadConfig-r12,

 t350-r12 ENUMERATED {min5, min10, min20, min30, min60,

 min120, min180, spare1} OPTIONAL -- Need OR

 }

 } OPTIONAL, -- Need ON

 scg-Configuration-r12 SCG-Configuration-r12 OPTIONAL, -- Cond nonFullConfig

 sl-SyncTxControl-r12 SL-SyncTxControl-r12 OPTIONAL, -- Need ON

 sl-DiscConfig-r12 SL-DiscConfig-r12 OPTIONAL, -- Need ON

 sl-CommConfig-r12 SL-CommConfig-r12 OPTIONAL, -- Need ON

 nonCriticalExtension RRCConnectionReconfiguration-v1310-IEs OPTIONAL

}

RRCConnectionReconfiguration-v1310-IEs ::= SEQUENCE {

 sCellToReleaseListExt-r13 SCellToReleaseListExt-r13 OPTIONAL, -- Need ON

 sCellToAddModListExt-r13 SCellToAddModListExt-r13 OPTIONAL, -- Need ON

 lwa-Configuration-r13 LWA-Configuration-r13 OPTIONAL, -- Need ON

 lwip-Configuration-r13 LWIP-Configuration-r13 OPTIONAL, -- Need ON

 rclwi-Configuration-r13 RCLWI-Configuration-r13 OPTIONAL, -- Need ON

 nonCriticalExtension RRCConnectionReconfiguration-v1430-IEs OPTIONAL

}

RRCConnectionReconfiguration-v1430-IEs ::= SEQUENCE {

 sl-V2X-ConfigDedicated-r14 SL-V2X-ConfigDedicated-r14 OPTIONAL, -- Need ON

 sCellToAddModListExt-v1430 SCellToAddModListExt-v1430 OPTIONAL, -- Need ON

 perCC-GapIndicationRequest-r14 ENUMERATED{true} OPTIONAL, -- Need ON

 systemInformationBlockType2Dedicated-r14 OCTET STRING (CONTAINING SystemInformationBlockType2) OPTIONAL, -- Cond nonHO

 nonCriticalExtension RRCConnectionReconfiguration-v1510-IEs OPTIONAL

}

RRCConnectionReconfiguration-v1510-IEs ::= SEQUENCE {

 nr-Config-r15 CHOICE {

 release NULL,

 setup SEQUENCE {

 endc-ReleaseAndAdd-r15 BOOLEAN,

 nr-SecondaryCellGroupConfig-r15 OCTET STRING OPTIONAL, -- Need ON

 p-MaxEUTRA-r15 P-Max OPTIONAL -- Need ON

 }

 } OPTIONAL, -- Need ON

 sk-Counter-r15 INTEGER (0.. 65535) OPTIONAL, -- Need ON

 nr-RadioBearerConfig1-r15 OCTET STRING OPTIONAL, -- Need ON

 nr-RadioBearerConfig2-r15 OCTET STRING OPTIONAL, -- Need ON

 tdm-PatternConfig-r15 CHOICE {

 release NULL,

 setup SEQUENCE {

 subframeAssignment-r15 SubframeAssignment-r15,

 harq-Offset-r15 INTEGER (0.. 9)

 }

 } OPTIONAL, -- Cond FDD-PCell

 nonCriticalExtension RRCConnectionReconfiguration-v1530-IEs OPTIONAL

}

RRCConnectionReconfiguration-v1530-IEs ::= SEQUENCE {

 securityConfigHO-v1530 SecurityConfigHO-v1530 OPTIONAL, -- Cond HO-5GC

 sCellGroupToReleaseList-r15 SCellGroupToReleaseList-r15 OPTIONAL, -- Need ON

 sCellGroupToAddModList-r15 SCellGroupToAddModList-r15 OPTIONAL, -- Need ON

 dedicatedInfoNASList-r15 SEQUENCE (SIZE(1..maxDRB-r15)) OF

 DedicatedInfoNAS OPTIONAL, -- Cond nonHO

 p-MaxUE-FR1-r15 P-Max OPTIONAL, -- Need OR

 smtc-r15 MTC-SSB-NR-r15 OPTIONAL, -- Need OP

 nonCriticalExtension SEQUENCE {} OPTIONAL

}

<Skip unrelated Parts>

-- ASN1STOP

| *RRCConnectionReconfiguration* field descriptions |
| --- |
| ***dedicatedInfoNASList***This field is used to transfer UE specific NAS layer information between the network and the UE. The RRC layer is transparent for each PDU in the list. If *dedicatedInfoNASList-r15* is present, UE shall ignore the *dedicatedInfoNASList* (without suffix). |
| ***endc-ReleaseAndAdd***A one-shot field indicating whether the UE simultaneously releases and adds all the NR SCG related configuration within *nr-Config*, i.e. the configuration set by the NR *RRCReconfiguration* message (e.g. *secondaryCellGroup, SRB3* and *measConfig)*. |
| ***fullConfig***Indicates the full configuration option is applicable for the RRC Connection Reconfiguration message. |
| ***harq-Offset***Indicates a HARQ subframe offset that is applied to the subframes designated as UL in the associated subrame assignment, see TS 36.213 [23]. |
| ***keyChangeIndicator***If UE is connected to EPC, true is used only in an intra-cell handover when a KeNB key is derived from a KASME key taken into use through the latest successful NAS SMC procedure, as described in TS 33.401 [32] for KeNB re-keying. false is used in an intra-LTE handover when the new KeNB key is obtained from the current KeNB key or from the NH as described in TS 33.401 [32].If UE is connected to 5GC, with keyChangeIndicator-r15, true is used in an intra-cell handover when a KeNB key is derived from a KAMF key taken into use through the latest successful NAS SMC procedure, as described in TS 33.501 [86] for KeNB re-keying.False is used for intra-system handover when the new KeNB key is obtained from the current KeNB key or from the NH as described in TS 33.501 [86]. True is also used in NG based handover procedure with KAMF change, when a KeNB key is derived from the new KAMF key as described in TS 33.501 [86]. |
| ***lwa-Configuration***This field is used to provide parameters for LWA configuration. E-UTRAN does not simultaneously configure LWA with DC, LWIP or RCLWI for a UE. |
| ***lwip-Configuration***This field is used to provide parameters for LWIP configuration. E-UTRAN does not simultaneously configure LWIP with DC, LWA or RCLWI for a UE. |
| ***nas-Container***This field is used to transfer UE specific NAS layer information between the network and the UE. The RRC layer is transparent for this field, although, if included, it affects activation of AS- security after handover within E-UTRA/5GC. The content is defined in TS 24.501 [95]. In case of NG based handover, the content of nas-Container is. the Intra N1 mode NAS transparent container IE. In case of inter-system handover to from 5GS to EPS, the content of NAS-Container is. the S1 mode to N1 mode NAS transparent container IE. |
| ***nas-securityParamToEUTRA***This field is used to transfer UE specific NAS layer information between the network and the UE. The RRC layer is transparent for this field, although, if included, it affects activation of AS- security after inter-RAT handover to E-UTRA/EPC or inter-system handover to E-UTRA/EPC. The content is defined in TS 24.301 [35]. This field is not used for handover from 5GC. |
| ***networkControlledSyncTx***This field indicates whether the UE shall transmit synchronisation information (i.e. become synchronisation source). Value *On* indicates the UE to transmit synchronisation information while value *Off* indicates the UE to not transmit such information. |
| ***nextHopChainingCount***Parameter NCC: See TS 33.401 [32] if UE is connected to EPC, else see 33.501 [86] if UE is connected to 5GC. |
| ***nr-Config***Includes the NR related configurations. This filed is used to configure EN-DC configuration, possibly in conjunction with fields *sk-Counter* and *nr-RadioBearerConfig1/ 2*. NOTE. |
| ***nr-RadioBearerConfig1, nr-RadioBearerConfig2***Includes the NR *RadioBearerConfig* IE as specified in TS 38.331 [82]. The field includes the configuration of RBs configured with NR PDCP. |
| ***nr-SecondaryCellGroupConfig***Includes the NR *RRCReconfiguration* message as specified in TS 38.331 [82]. In this version of the specification, the NR RRC message only includes fields *secondaryCellGroup* and/ or *measConfig*. If *nr-SecondaryCellGroupConfig* is configured, the network always includes this field upon MN handover to initiate an NR SCG reconfiguration with sync and key change. |
| ***perCC-GapIndicationRequest***Indicates that UE shall include *perCC-GapIndicationList* and *numFreqEffective* in the *RRCConnectionReconfigurationComplete* message. *numFreqEffectiveReduced* may also be included if frequencies are configured for reduced measurement performance. |
| ***p-MaxEUTRA***Indicates the maximum power available for LTE. |
| ***p-MaxUE-FR1***The maximum total transmit power to be used by the UE across all serving cells in frequency range 1 (FR1) across all cell groups. The maximum transmit power that the UE may use may be additionally limited on cell- or cell-group level. The field is optionally present, if EN-DC (nr-Config-r15) has been configured. It is absent otherwise. |
| ***p-MeNB***Indicates the guaranteed power for the MeNB, as specified in TS 36.213 [23]. The value N corresponds to N-1 in TS 36.213 [23]. |
| ***powerControlMode***Indicates the power control mode used in DC. Value 1 corresponds to DC power control mode 1 and value 2 indicates DC power control mode 2, as specified in TS 36.213 [23]. |
| ***p-SeNB***Indicates the guaranteed power for the SeNB as specified in TS 36.213 [23, Table 5.1.4.2-1]. The value N corresponds to N-1 in TS 36.213 [23]. |
| ***rclwi-Configuration***WLAN traffic steering command as specified in 5.6.16.2. E-UTRAN does not simultaneously configure RCLWI with DC, LWA or LWIP for a UE. |
| ***sCellConfigCommon***Indicates the common configuration for the SCell group. |
| ***sCellGroupIndex***Indicates the identity of SCell groups for which a common configuration is provided. |
| ***sCellIndex***In case of DC, the SCellIndex is unique within the scope of the UE i.e. an SCG cell can not use the same value as used for an MCG cell. For *pSCellToAddMod*, if *sCellIndex-r13* is present the UE shall ignore *sCellIndex-r12.* *sCellIndex-r13* in *sCellToAddModListExt-r13* shall not have same values as sCellIndex-r10 in sCellToAddModList-r10. |
| ***sCellGroupToAddModList, sCellGroupToAddModListSCG***Indicates the SCell group to be added or modified. E-UTRAN only configures at most 4 SCell groups per UE over all cell groups. |
| ***sCellGroupToReleaseList***Indicates the SCell group to be released. |
| ***sCellState***A one-shot field that indicates whether the SCell shall be considered to be in activated or dormant state upon SCell configuration. |
| ***sCellToAddModList, sCellToAddModListExt***Indicates the SCell to be added or modified. Field *sCellToAddModList* is used to add the first 4 SCells for a UE with *sCellIndex-r10* while *sCellToAddModListExt* is used to add the rest. If E-UTRAN includes *sCellToAddModListExt-v1430* it includes the same number of entries, and listed in the same order, as in *sCellToAddModListExt-r13*. If E-UTRAN includes *sCellToAddModList-v10l0* it includes the same number of entries, and listed in the same order, as in *sCellToAddModList-r10*. If E-UTRAN includes *sCellToAddModListExt-v1370* it includes the same number of entries, and listed in the same order, as in *sCellToAddModListExt-r13*. If E-UTRAN includes s*CellToAddModListExt-v13c0* it includes the same number of entries, and listed in the same order, as in s*CellToAddModListExt-r13.* |
| ***sCellToAddModListSCG, sCellToAddModListSCG-Ext***Indicates the SCG cell to be added or modified. The field is used for SCG cells other than the PSCell (which is added/ modified by field *pSCellToAddMod*). Field *sCellToAddModListSCG* is used to add the first 4 SCells for a UE with *sCellIndex-r10* while *sCellToAddModListSCG-Ext* is used to add the rest. If E-UTRAN includes *sCellToAddModListSCG-v10l0* it includes the same number of entries, and listed in the same order, as in *sCellToAddModListSCG-r12*. If E-UTRAN includes *sCellToAddModListSCG-Ext-v1370* it includes the same number of entries, and listed in the same order, as in *sCellToAddModListSCG-Ext-r13*. If E-UTRAN includes *sCellToAddModListSCG-Ext-v13c0* it includes the same number of entries, and listed in the same order, as in *sCellToAddModListSCG-Ext-r13.* |
| ***sCellToReleaseListSCG, sCellToReleaseListSCG-Ext***Indicates the SCG cell to be released. The field is also used to release the PSCell e.g. upon change of PSCell, upon system information change for the PSCell. |
| ***scg-Counter***A counter used upon initial configuration of SCG security as well as upon refresh of S-KeNB. E-UTRAN includes the field upon SCG change when one or more SCG DRBs are configured. Otherwise E-UTRAN does not include the field. |
| ***securityConfigHO***This field contains the parameters required to update the security keys at handover. If E-UTRAN includes the *securityConfigHO* (i.e., without suffix), the choice *intraLTE* is used for handover within E-UTRA/EPC while the choice *interRAT* is used for handover from GERAN or UTRAN to E-UTRA/EPC. If E-UTRAN includes the *securityConfigHO-v1530* (i.e., with suffix), the choice *intra5GC* is used for handover from NR or E-UTRA/5GC to E-UTRA/5GC while the choice *ngc-ToEPC* is used for inter-system handover from NR or E-UTRA/5GC to E-UTRA/EPC and the choice *epc-ToNGC* is used for inter-system handover from E-UTRA/EPC to E-UTRA/5GC. |
| ***sk-Counter***A one-shot counter used upon initial configuration of security for EN-DC as well as upon refresh of S-KgNB. E-UTRAN provides this field upon configuring EN-DC to facilitate configuration of SRB3. |
| ***sl-V2X-ConfigDedicated***Indicates sidelink configuration for non-P2X related V2X sidelink communication as well as P2X related V2X sidelink communication. |
| ***smtc***The SSB periodicity/offset/duration configuration of target NR PSCell for NR PSCell addition and SN change. If the EUTRA PCell is changed within the same *RRCConnectionReconfiguration* message (i.e. intra-LTE handover), the timing reference is target EUTRA PCell. For all other cases, the timing reference is the EUTRA PCell. If the field is absent, the UE uses the SMTC configured in the *measObjectNR* having the same SSB frequency and subcarrier spacing. |
| ***srs-SwitchFromServCellIndex***Indicates the serving cell whose UL transmission may be interrupted during SRS transmission on a PUSCH-less cell. During SRS transmission on a PUSCH-less cell, the UE may temporarily suspend the UL transmission on a serving cell with PUSCH in the same CG to allow the PUSCH-less cell to transmit SRS. The PUSCH-less cell is always a TDD cell but the serving cell with PUSCH may be either a FDD or TDD cell. |
| ***subframeAssignment***Indicates DL/UL subframe configuration where sa0 points to Configuration 0, sa1 to Configuration 1 etc. as specified in TS 36.211 [21, table 4.2-2]. |
| ***systemInformationBlockType1Dedicated***This field is used to transfer *SystemInformationBlockType1* or *SystemInformationBlockType1-BR* to the UE. |
| ***systemInformationBlockType2Dedicated***This field is used to transfer BR version of *SystemInformationBlockType2* to BL UEs or UEs in CE or *SystemInformationBlockType2* to non-BL UEs. |
| ***t350***Timer T350 as described in section 7.3. Value *minN* corresponds to N minutes. |
| ***tdm-PatternConfig***UL/DL reference configuration indicating the time during which a UE configured with EN-DC is allowed to transmit. This field is used when power control or IMD issues require single UL transmission as specified in TS38.101-3 [85] and TS 38.213 [88]. |