**3GPP TSG-RAN2 Meeting #107bis R2-19xxxxx**

**Chongqing, China, 14th – 18th Oct, 2019**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.0* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **37.324** | **CR** | **DraftCR** | **rev** | **-** | **Current version:** | **15.1.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network | **X** | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Running CR to 37324 for 5G\_V2X\_NRSL | | | | | | | | | |
|  |  | | | | | | | | | |
|  |  | | | | | | | | | |
|  |  | | | | | | | | | |
|  |  | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | R2 | | | | | | | | | |
| ***Source to TSG:*** | Rapporteur (vivo) | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | 5G\_V2X\_NRSL-Core | | | | |  | ***Date:*** | | | 2019-10-24 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **B** |  | | | | | ***Release:*** | | | Rel-16 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) Rel-12 (Release 12)* *Rel-13 (Release 13) Rel-14 (Release 14) Rel-15 (Release 15) Rel-16 (Release 16)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | This CR is to capture the following agreements related to SDAP for the 5G\_V2X\_NRSL-Core WI:  **RAN2#105 agreements:**   * SDAP layer is needed at least for SL unicast, performing PC5 QoS flow to SLRB mapping. SDAP layer is not needed for per-packet QoS model, e.g. broadcast.   **RAN2#106 agreements:**   * No need of reflective QoS.   **RAN2#107bis agreements:**   * SDAP layer is supported for NR SL groupcast and broadcast. * For NR SL unicast, groupcast and broadcast, PDU session concept/PDU session ID is not supported by SDAP sublayer. * SDAP entity is configured per destination L2 id and cast type in the UE. * For NR SL unicast Tx and Rx SDAP entity, both establishment and release are requested by upper layers (i.e., follow NR Uu as baseline). * For NR SL groupcast and broadcast Tx SDAP entity, both establishment and release are requested by upper layers (i.e., follow NR Uu as baseline). * For all casts, RDI field is not supported in NR SL SDAP PDU header. * For NR SL unicast, in order delivery in case of remapping is achieved by using SDAP PDU with header (Using end marker). * For NR SL unicast, no enhancement for Rx behavior to be specified compared to Uu solution. FFS whether the Rx behavior is left to UE implementation. * For NR SL groupcast and broadcast, in order delivery in case of remapping is achieved by Tx side implementation and only the SDAP PDU format without header will be used. * For NR SL Unicast, QFI/PFI (PC5 Flow ID) field is supported in NR SL SDAP PDU header. Note: In Rel-16 in case this field is present, it is only used for QoS flow to SLRB remapping. * For NR SL unicast D/C field is supported in NR SL SDAP PDU header. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Capture RAN2 agreements | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | If the CR is not approved, the NR V2X will not be specified in the SDAP 37.324 specification. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 2, 3.1, 3.2, 4.2.1, 4.2.2, 4.4, 5.1.1, 5.1.2, 5.2.1a, 5.2.2a, 5.3, 5.3.1, 5.3.3, 6.2.2, 6.3.4 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | | This draftCR is based on the version 15.1.0 of 37.324. | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

3GPP TS 37.324 V15.1.0 (2018-09)

Technical Specification

**3rd Generation Partnership Project;**

**Technical Specification Group Radio Access Network;**

E-UTRA and NR;

**Service Data Adaptation Protocol (SDAP) specification**

(Release 15)

** 

The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP..  
The present document has not been subject to any approval process by the 3GPPOrganizational Partners and shall not be implemented.  
This Specification is provided for future development work within 3GPPonly. The Organizational Partners accept no liability for any use of this Specification.  
Specifications and Reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organizational Partners' Publications Offices.

***3GPP***

Postal address

3GPP support office address

650 Route des Lucioles - Sophia Antipolis

Valbonne - FRANCE

Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16

Internet

http://www.3gpp.org

***Copyright Notification***

No part may be reproduced except as authorized by written permission.  
The copyright and the foregoing restriction extend to reproduction in all media.

© 2018, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

UMTS™ is a Trade Mark of ETSI registered for the benefit of its members

3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  
LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners

GSM® and the GSM logo are registered and owned by the GSM Association

Contents

Foreword 4

1 Scope 5

2 References 5

3 Definitions, symbols and abbreviations 5

3.1 Definitions 5

3.2 Abbreviations 5

4 General 6

4.1 Introduction 6

4.2 SDAP architecture 6

4.2.1 SDAP structure 6

4.2.2 SDAP entities 6

4.3 Services 7

4.3.1 Services provided to upper layers 7

4.3.2 Services expected from lower layers 7

4.4 Functions 8

5 SDAP procedures 8

5.1 SDAP entity handling 8

5.1.1 SDAP entity establishment 8

5.1.2 SDAP entity release 8

5.2 Data transfer 8

5.2.1 Uplink 8

5.2.2 Downlink 9

5.3 QoS flow to DRB mapping 9

5.3.1 Configuration 9

5.3.2 Reflective mapping 9

5.3.3 DRB release 10

5.4 RQI handling 10

6 Protocol data units, formats, and parameters 10

6.1 Protocol data units 10

6.1.1 Data PDU 10

6.1.2 Control PDU 10

6.2 Formats 10

6.2.1 General 10

6.2.2 Data PDU 11

6.2.2.1 Data PDU without SDAP header 11

6.2.2.2 DL Data PDU with SDAP header 11

6.2.2.3 UL Data PDU with SDAP header 11

6.2.3 End-Marker Control PDU 11

6.3 Parameters 12

6.3.1 General 12

6.3.2 Data 12

6.3.3 D/C 12

6.3.4 QFI 12

6.3.5 R 12

6.3.6 RQI 12

6.3.7 RDI 13

Annex A (informative): Change history 13

# Foreword

This Technical Specification has been produced by the 3rd Generation Partnership Project (3GPP).

The contents of the present document are subject to continuing work within the TSG and may change following formal TSG approval. Should the TSG modify the contents of the present document, it will be re-released by the TSG with an identifying change of release date and an increase in version number as follows:

Version x.y.z

where:

x the first digit:

1 presented to TSG for information;

2 presented to TSG for approval;

3 or greater indicates TSG approved document under change control.

y the second digit is incremented for all changes of substance, i.e. technical enhancements, corrections, updates, etc.

z the third digit is incremented when editorial only changes have been incorporated in the document.

# 1 Scope

The present document specifies the Service Data Adaptation Protocol (SDAP) for a UE with connection to the 5G-CN.

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications".

[2] 3GPP TS 38.300: "NG Radio Access Network; Overall description".

[3] 3GPP TS 38.331: "NR Radio Resource Control (RRC); Protocol Specification".

[4] 3GPP TS 23.501: "System Architecture for the 5G System".

[X] 3GPP TS 23.287: "Architecture enhancements for 5G System (5GS) to support Vehicle-to-Everything (V2X) services".

# 3 Definitions, symbols and abbreviations

## 3.1 Definitions

For the purposes of the present document, the terms and definitions given in 3GPP TR 21.905 [1] and the following apply. A term defined in the present document takes precedence over the definition of the same term, if any, in 3GPP TR 21.905 [1].

**PC5 QoS flow to SL DRB mapping rule**: a mapping rule determining on which SL DRB packets of a PC5 QoS flow shall be carried.

**QoS flow to DRB mapping rule**: a mapping rule determining on which DRB packets of a QoS flow shall be carried.

**Reflective QoS flow to DRB mapping**: a QoS flow to DRB mapping scheme where a UE monitors the QoS flow to DRB mapping rule in the DL, and applies it to in the UL.

**NR Sidelink communication**: AS functionality enabling at least V2X communication as defined in TS 23.287 [X], between two or more nearby UEs, using NR technology but not traversing any network node.

## 3.2 Abbreviations

For the purposes of the present document, the abbreviations given in 3GPP TR 21.905 [1] and the following apply. An abbreviation defined in the present document takes precedence over the definition of the same abbreviation, if any, in 3GPP TR 21.905 [1].

PFI PC5 QoS Flow ID

QFI QoS Flow ID

RDI Reflective QoS flow to DRB mapping Indication

RQI Reflective QoS Indication

SDAP Service Data Adaptation Protocol

SL Sidelink

SL DRB Sidelink Data Radio Bearer carrying NR Sidelink communication data

# 4 General

## 4.1 Introduction

The objective is to describe the SDAP architecture and the SDAP entity from a functional point of view. The specified functionality only applies to UE with connection to the 5G-CN and UE in SL unicast, groupcast or broadcast communications.

## 4.2 SDAP architecture

### 4.2.1 SDAP structure

Figure 4.2.1-1 illustrates one possible structure for the SDAP sublayer; it should not restrict implementation. The figure is based on the radio interface protocol architecture defined in 3GPP TS 38.300 [2].



Figure 4.2.1-1: SDAP sublayer, structure view

The SDAP sublayer is configured by RRC (3GPP TS 38.331 [3]). The SDAP sublayer maps QoS flows to DRBs. One or more QoS flows may be mapped onto one DRB. One QoS flow is mapped onto only one DRB at a time in the UL.

In SL communication, the SDAP sublayer maps PC5 QoS flows to SL DRBs. One or more PC5 QoS flows may be mapped onto one SL DRB. One PC5 QoS flow is mapped onto only one SL DRB at a time in the SL.

### 4.2.2 SDAP entities

The SDAP entities are located in the SDAP sublayer. Several SDAP entities may be defined for a UE. There is an SDAP entity configured for each individual PDU session. For SL, SDAP entity is configured per destination Layer2 identity and cast type in the UE.

An SDAP entity receives/delivers SDAP SDUs from/to upper layers and submits/receives SDAP data PDUs to/from its peer SDAP entity via lower layers.

- At the transmitting side, when an SDAP entity receives an SDAP SDU from upper layers, it constructs the corresponding SDAP data PDU and submits it to lower layers;

- At the receiving side, when an SDAP entity receives an SDAP data PDU from lower layers, it retrieves the corresponding SDAP SDU and delivers it to upper layers.

Figure 4.2.2-1 illustrates the functional view of the SDAP entity for the SDAP sublayer; it should not restrict implementation. The figure is based on the radio interface protocol architecture defined in 3GPP TS 38.300 [2].



Figure 4.2.2-1: SDAP layer, functional view

Reflective QoS flow to DRB mapping is performed at UE, as specified in the subclause 5.3.2, if DL SDAP header is configured.

For SL communication, reflective PC5 QoS flow to SL DRB mapping is not supported.

## 4.3 Services

### 4.3.1 Services provided to upper layers

The SDAP sublayer provides its service to the user plane upper layers. The following services are provided by SDAP to upper layers:

- transfer of user plane data.

### 4.3.2 Services expected from lower layers

An SDAP entity expects the following services from lower layers:

- user plane data transfer service;

- in-order delivery except when out of order delivery is configured by RRC (3GPP TS 38.331 [3]).

## 4.4 Functions

The SDAP sublayer supports the following functions:

- transfer of user plane data;

- mapping between a QoS flow and a DRB for both DL and UL;

- mapping between a PC5 QoS flow and a SL DRB for SL;

- marking QoS flow ID in both DL and UL packets;

- reflective QoS flow to DRB mapping for the UL SDAP data PDUs.

# 5 SDAP procedures

## 5.1 SDAP entity handling

### 5.1.1 SDAP entity establishment

When RRC (3GPP TS 38.331 [3]) requests an SDAP entity establishment, the UE shall:

- establish an SDAP entity;

- follow the procedures in subclause 5.2.

When upper layer (3GPP TS 38.331 [3]) requests establishment of an SL unicast transmitting or receiving SDAP entity or an SL groupcast and broadcast transmitting SDAP entity, the UE shall:

- establish an SDAP entity;

- follow the procedures in subclause 5.2.

### 5.1.2 SDAP entity release

When RRC (3GPP TS 38.331 [3]) requests an SDAP entity release, the UE shall:

- release the SDAP entity.

When upper layer (3GPP TS 38.331 [3]) requests release an SL unicast transmitting or receiving SDAP entity or an SL groupcast and broadcast transmitting SDAP entity, the UE shall:

- release the SDAP entity.

## 5.2 Data transfer

### 5.2.1 Uplink

At the reception of an SDAP SDU from upper layer for a QoS flow, the transmitting SDAP entity shall:

- if there is no stored QoS flow to DRB mapping rule for the QoS flow as specified in the subclause 5.3:

- map the SDAP SDU to the default DRB;

- else:

- map the SDAP SDU to the DRB according to the stored QoS flow to DRB mapping rule;

- if the DRB to which the SDAP SDU is mapped is configured by RRC (3GPP TS 38.331 [3]) with the presence of SDAP header,

- construct the UL SDAP data PDU as specified in the subclause 6.2.2.3;

- else:

- construct the UL SDAP data PDU as specified in the subclause 6.2.2.1;

- submit the constructed UL SDAP data PDU to the lower layers.

NOTE 1: UE behaviour is not defined if there is neither a default DRB nor a stored QoS flow to DRB mapping rule for the QoS flow.

NOTE 2: Default DRB is always configured with UL SDAP header (3GPP TS 38.331 [3]).

### 5.2.2 Downlink

At the reception of an SDAP data PDU from lower layers for a QoS flow, the receiving SDAP entity shall:

- if the DRB from which this SDAP data PDU is received is configured by RRC (3GPP TS 38.331 [3]) with the presence of SDAP header:

- perform reflective QoS flow to DRB mapping as specified in the subclause 5.3.2;

- perform RQI handling as specified in the subclause 5.4;

- retrieve the SDAP SDU from the DL SDAP data PDU as specified in the subclause 6.2.2.2.

- else:

- retrieve the SDAP SDU from the DL SDAP data PDU as specified in the subclause 6.2.2.1;

- deliver the retrieved SDAP SDU to the upper layer.

### 5.2.X SL transmission

At the reception of an SDAP SDU from upper layer for a PC5 QoS flow, the transmitting SDAP entity shall:

- if there is no stored PC5 QoS flow to SL DRB mapping rule for the PC5 QoS flow as specified in the subclause 5.3:

- map the SDAP SDU to the default SL DRB;

- else:

- map the SDAP SDU to the SL DRB according to the stored PC5 QoS flow to SL DRB mapping rule;

- if the SL DRB to which the SDAP SDU is mapped is configured by RRC (3GPP TS 38.331 [3]) with the presence of SDAP header,

- construct the SL SDAP data PDU as specified in the subclause 6.2.2.4;

- else:

- construct the SL SDAP data PDU as specified in the subclause 6.2.2.1;

- submit the constructed SL SDAP data PDU to the lower layers.

### 5.2.Y SL reception

At the reception of an SDAP data PDU from lower layers for a PC5 QoS flow, the receiving SDAP entity shall:

- if the SL DRB from which this SDAP data PDU is received is configured by RRC (3GPP TS 38.331 [3]) with the presence of SDAP header:

- retrieve the SDAP SDU from the SL SDAP data PDU as specified in the subclause 6.2.2.4.

- else:

- retrieve the SDAP SDU from the SL SDAP data PDU as specified in the subclause 6.2.2.1;

- deliver the retrieved SDAP SDU to the upper layer.

Editor's Notes: FFS whether the receiver behavior upon remapping is left to UE implementation

## 5.3 QoS flow to DRB mapping

### 5.3.1 Configuration

When RRC (3GPP TS 38.331 [3]) configures an UL QoS flow to DRB mapping rule for a QoS flow, the SDAP entity shall:

- if the SDAP entity has already been established and there is no stored QoS flow to DRB mapping rule for the QoS flow and a default DRB is configured:

- construct an end-marker control PDU, as specified in the subclause 6.2.3, for the QoS flow;

- map the end-marker control PDU to the default DRB;

- submit the end-marker control PDU to the lower layers.

- if the stored UL QoS flow to DRB mapping rule is different from the configured QoS flow to DRB mapping rule for the QoS flow and the DRB according to the stored QoS flow to DRB mapping rule is configured by RRC (3GPP TS 38.331 [3]) with the presence of UL SDAP header:

- construct an end-marker control PDU, as specified in the subclause 6.2.3, for the QoS flow;

- map the end-marker control PDU to the DRB according to the stored QoS flow to DRB mapping rule;

- submit the end-marker control PDU to the lower layers.

- store the configured UL QoS flow to DRB mapping rule for the QoS flow.

When RRC (3GPP TS 38.331 [3]) releases an UL QoS flow to DRB mapping rule for a QoS flow, the SDAP entity shall:

- remove the UL QoS flow to DRB mapping rule for the QoS flow.

### 5.3.2 Reflective mapping

For each received DL SDAP data PDU with RDI set to 1, the SDAP entity shall:

- process the QFI field in the SDAP header and determine the QoS flow;

- if there is no stored QoS flow to DRB mapping rule for the QoS flow and a default DRB is configured:

- construct an end-marker control PDU, as specified in the subclause 6.2.3, for the QoS flow;

- map the end-marker control PDU to the default DRB;

- submit the end-marker control PDU to the lower layers;

- if the stored QoS flow to DRB mapping rule for the QoS flow is different from the QoS flow to DRB mapping of the DL SDAP data PDU and the DRB according to the stored QoS flow to DRB mapping rule is configured by RRC (3GPP TS 38.331 [3]) with the presence of UL SDAP header:

- construct an end-marker control PDU, as specified in the subclause 6.2.3, for the QoS flow;

- map the end-marker control PDU to the DRB according to the stored QoS flow to DRB mapping rule;

- submit the end-marker control PDU to the lower layers;

- store the QoS flow to DRB mapping of the DL SDAP data PDU as the QoS flow to DRB mapping rule for the UL.

### 5.3.3 DRB release

When RRC (3GPP TS 38.331 [3]) indicates that a DRB is released, the SDAP entity shall:

- remove all QoS flow to DRB mappings associated with the released DRB based on the subclauses 5.3.1 and 5.3.2.

## 5.4 RQI handling

For each received DL SDAP data PDU with RQI set to 1, the SDAP entity shall:

- inform the NAS layer of the RQI and QFI.

## 5.X PC5 QoS flow to SL DRB mapping

### 5.X.X Configuration

When RRC (3GPP TS 38.331 [3]) configures a PC5 QoS flow to SL DRB mapping rule for a PC5 QoS flow, the SDAP entity shall:

- for SL unicast, if the SDAP entity has already been established and there is no stored SL DRB mapping rule for the PC5 QoS flow and a default SL DRB is configured with the presence of SL SDAP header:

- construct an end-marker control PDU, as specified in the subclause 6.2.3, for the PC5 QoS flow;

- map the end-marker control PDU to the default SL DRB;

- submit the end-marker control PDU to the lower layers.

- for SL unicast, if the stored PC5 QoS flow to SL DRB mapping rule is different from the configured SL DRB mapping rule for the PC5 QoS flow and the SL DRB according to the stored PC5 QoS flow to SL DRB mapping rule is configured by RRC (3GPP TS 38.331 [3]) with the presence of SL SDAP header:

- construct an end-marker control PDU, as specified in the subclause 6.2.3, for the PC5 QoS flow;

- map the end-marker control PDU to the SL DRB according to the stored PC5 QoS flow to SL DRB mapping rule;

- submit the end-marker control PDU to the lower layers.

- store the configured PC5 QoS flow to SL DRB mapping rule for the PC5 QoS flow.

When RRC (3GPP TS 38.331 [3]) releases a PC5 QoS flow to SL DRB mapping rule for a PC5 QoS flow, the SDAP entity shall:

- remove the PC5 QoS flow to SL DRB mapping rule for the PC5 QoS flow.

### 5.X.Y SL DRB release

When RRC (3GPP TS 38.331 [3]) indicates that a SL DRB is released, the SDAP entity shall:

- remove all PC5 QoS flow to SL DRB mappings associated with the released SL DRB based on the subclauses 5.3.1 and 5.3.2.

# 6 Protocol data units, formats, and parameters

## 6.1 Protocol data units

### 6.1.1 Data PDU

The SDAP Data PDU is used to convey one or more of followings:

- SDAP header;

- user plane data.

### 6.1.2 Control PDU

a) End-Marker Control PDU

End-Marker control PDU is used by the SDAP entity at UE to indicate that it stops the mapping of the SDAP SDU of the QoS flow indicated by the QFI to the DRB on which the End-Marker PDU is transmitted.

## 6.2 Formats

### 6.2.1 General

A SDAP PDU is a bit string that is byte aligned (i.e. multiple of 8 bits) in length. In the figures in subclause 6.2, bit strings are represented by tables in which the first and most significant bit is the left most bit of the first line of the table, the last and least significant bit is the rightmost bit of the last line of the table, and more generally the bit string is to be read from left to right and then in the reading order of the lines.

SDAP SDUs are bit strings that are byte aligned (i.e. multiple of 8 bits) in length. An SDAP SDU is included into a SDAP PDU from the first bit onward.

For SL groupcast and broadcast, only SDAP data PDU without SDAP header is supported.

### 6.2.2 Data PDU

#### 6.2.2.1 Data PDU without SDAP header

An SDAP PDU consists only of a data field and does not consist of any SDAP header, as described in Figure 6.2.2.1-1.



Figure 6.2.2.1-1: SDAP Data PDU format without SDAP header

#### 6.2.2.2 DL Data PDU with SDAP header

Figure 6.2.2.2 – 1 shows the format of SDAP Data PDU of DL with SDAP header being configured.



Figure 6.2.2.2-1: DL SDAP Data PDU format with SDAP header

#### 6.2.2.3 UL Data PDU with SDAP header

Figure 6.2.2.3 – 1 shows the format of SDAP Data PDU of UL with SDAP header being configured.



Figure 6.2.2.3-1: UL SDAP Data PDU format with SDAP header

#### 6.2.2.4 SL Data PDU with SDAP header for SL unicast

Figure 6.2.2.4 – 1 shows the format of SDAP Data PDU of SL unicast with SDAP header being configured.



Figure 6.2.2.4-1: SL SDAP Data PDU format with SDAP header for SL unicast

### 6.2.3 End-Marker Control PDU

Figure 6.2.3 – 1 shows the format of End-Marker Control PDU.



Figure 6.2.3-1: End-Marker Control PDU

## 6.3 Parameters

### 6.3.1 General

If not otherwise mentioned in the definition of each field, then the bits in the parameters shall be interpreted as follows: the left most bit is the first and most significant bit and the right most bit is the last and least significant bit.

Unless otherwise mentioned, integers are encoded in standard binary encoding for unsigned integers. In all cases the bits appear ordered from MSB to LSB when read in the PDU.

### 6.3.2 Data

Length: Variable

This field includes the SDAP SDU.

### 6.3.3 D/C

Length: 1 bit,

The D/C bit indicates whether the SDAP PDU is an SDAP Data PDU or an SDAP Control PDU.

Table 6.3.3-1: D/C field

|  |  |
| --- | --- |
| Bit | Description |
| 0 | Control PDU |
| 1 | Data PDU |

### 6.3.4 QFI

Length: 6 bits

The QFI field indicates the ID of the QoS flow (3GPP TS 23.501 [4]) to which the SDAP PDU belongs.

### 6.3.5 R

Length: 1 bit

Reserved. In this version of the specification reserved bits shall be set to 0. Reserved bits shall be ignored by the receiver.

### 6.3.6 RQI

Length: 1 bit,

The RQI bit indicates whether NAS should be informed of the updated of SDF to QoS flow mapping rules (3GPP TS 23.501 [4]).

Table 6.3.6-1: RQI field

|  |  |
| --- | --- |
| Bit | Description |
| 0 | No action |
| 1 | To inform NAS that RQI bit is set to 1. |

### 6.3.7 RDI

Length: 1 bit,

The RDI bit indicates whether QoS flow to DRB mapping rule should be updated.

Table 6.3.7-1: RDI field

|  |  |
| --- | --- |
| Bit | Description |
| 0 | No action |
| 1 | To store QoS flow to DRB mapping rule. |

### 6.3.X PFI

Length: 6 bits

The PFI field indicates the ID of the PC5 QoS flow (3GPP TS 23.287[x]) to which the SDAP PDU belongs.

Annex A (informative):  
Change history

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Change history** | | | | | | | |
| **Date** | **Meeting** | **TDoc** | **CR** | **Rev** | **Cat** | **Subject/Comment** | **New version** |
| 06/2017 | RAN2 NR AH |  | - | - | - | First version | 0.1.0 |
| 08/2017 | RAN2#99 |  | - | - | - | To capture agreements made in RAN2#99 | 0.2.0 |
| 09/2017 | RAN#77 |  | - | - | - | Presented to RAN#77 for information | 1.0.0 |
| 10/2017 | RAN2#99bis |  |  |  |  | To capture agreements made in RAN2#99bis | 1.1.0 |
| 11/2017 | RAN2#100 |  |  |  |  | To remove editor's notes. | 1.2.0 |
| 01/2018 | RAN2 NR AH |  |  |  |  | To capture agreements made in RAN2 NR AH | 1.3.0 |
| 04/2018 | RAN2#101bis |  |  |  |  | To capture agreements made in RAN2#101 | 1.4.0 |
|  | RAN2#101bis |  |  |  |  | To capture agreements made in RAN2#101bis | 1.5.0 |
| 05/2018 | RAN2#102 |  |  |  |  | To capture agreements made in RAN2#102 | 1.6.0 |
| 06/2018 | RP-80 | RP-181256 |  |  |  | Provided to RAN #80 for approval | 2.0.1 |
|  | RP-80 | RP-181266 |  |  |  | Provided to RAN #80 for approval (update as RP-181256 was misused for another Tdoc) | 2.0.2 |
|  |  |  |  |  |  | Upgraded to Rel-15 after the plenary approval | 15.0.0 |
| 09/2018 | RP-81 | RP-181940 | 0006 | 1 | F | Miscellaneous corrections for SDAP | 15.1.0 |
|  | RP-81 | RP-181939 | 0007 | - | D | Miscellaneous corrections to SDAP | 15.1.0 |
|  | RP-81 | RP-181942 | 0008 | 1 | F | Correction on flow remapping from default DRB | 15.1.0 |