3GPP TSG-RAN WG2 #116bis-e Tdoc R2-21xxxxx

Electronic meeting, 2022-01-17 - 2022-01-25

Agenda Item: 8.11.1

Source: Ericsson

Title: 38.331 RAT-dependent positioning running CR (Ericsson)

Document for: Discussion, Decision

# 1 Introduction

# 1 Introduction

This document is to collect comments for the following email discussion:

* [Post116bis-e][631][POS] 38.331 RAT-dependent positioning running CR (Ericsson)

      Scope: Check and endorse the running CR considering decisions of RAN2#116bis-e.

      Intended outcome: Endorsed CR

      Deadline:  Friday 2022-01-28 0800 UTC

# 2 Contact Information

|  |  |
| --- | --- |
| Company | Contact: Name (E-mail) |
| Intel | Yi guo (yi.guo@intel.com) |
| vivo | Xiang Pan (panxiang@vivo.com) |
| OPPO | Xin You(youxin@oppo.com) |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

# 3 Comments

**Please provide the comments on the CR here:**

|  |  |
| --- | --- |
| Company | Comments |
| Intel |  srs-PosRRC-InactiveConfig-r17 SRS-PosRRC-InactiveConfig-r17 OPTIONAL -- Need RSRS-PosRRC-InactiveConfig-r17 ::= SEQUENCE { srs-Config-r17 SRS-Config OPTIONAL, -- Need R bwp-r17 BWP OPTIONAL, -- Need R srs-TimeAlignmentTimer-r17 ENUMERARED {FFS align with SDT} OPTIONAL, -- Need R increaseThresh-r17 RSRP-ChangeThresh-r17, decreaseThresh-r17 RSRP-ChangeThresh-r16 OPTIONAL -- Need R}5.X  Timing alignment validation for SRS for Positioning transmission in RRC Inactive |
| vivo | Tend to capture the description related to validity determination in MAC (i.e., 38.321) and refine or remove 5.X.Regarding the UE behavior upon initiation of the RRC resume procedure, suggest the following description:1> if the UE has stored *srs-PosRRC-InactiveConfig*: 2> if the resume procedure is initiated in a cell that is different from the cell in which the UE received the stored *srs-PosRRC-InactiveConfig*: 3> release the stored *srs-PosRRC-InactiveConfig*;Besides, introduce the following RRC behavior to align with MAC behavior when TA timer expires:Upon receiving a positioning SRS configuration for RRC\_INACTIVE release request from lower layers, the UE shall:1. release the stored *srs-PosRRC-InactiveConfig*.

Regarding the ASN.1:We are wondering whether a single RSRP threshold is enough, that is, the configuration is considered to be valid when the RSRP ranges from RSRP0-threshold to RSRP0+threshold.Also, we would like to ask if other RRC related changes are discussed in this post email discussion in addition to the pos SRS for RRC\_INACTIVE? |
| OPPO | * The following agreement has not been capatured, SRS configuration as well as TA timer (*SRS-PosRRC-InactiveConfig*) should be released upon RRC resume is initiated for SDT in another cell.

*Proposal 4 When cell reselection is performed and UE initiates RRC resume procedure to the cell which is different from the cell in which the SRSp is configured, the TA timer configuration for SRS should be released.**Proposal 5 (modified) The SRSp configuration is released when the UE sends RRCResumeRequest to a cell other than the cell where it is released to RRC\_INACTIVE state.** For the RSRP threshold, we prefer to align with SDT CR, i.e. single RSRP threshold is configured.
 |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

# Conclusion

In the previous sections we made the following observations: