**3GPP TSG-RAN WG2 Meeting #116bis electronic R2-22xxxxx**

**Online, 17 – 25 January 2022**

**Source: vivo**

**Title:** **Summary of [POST116bis-e][706][V2X/SL] Open issues on power-saving resource allocation, Phase 1**

**Agenda Item:** **8.15.3**

**Document for:** **Discussion and Decision**

# Introduction

This contribution summarizes the Phase-1 discussion on open issue list review of the following email discussion:

* [POST116bis-e][706][V2X/SL] Open issues on power-saving resource allocation (vivo)

 **Scope:** 1st phase: Make an open issue lists with the proposed candidate options or rapporteur suggestion. Open issue lists can include pre-identified issues (e.g. FFS, not decided or skipped from previous offline/email discussion) and new issues raised in company contributions at RAN2#116bis. For new issues that have not discussed before, rapporteur can collect companies’ inputs (e.g. whether it is essential issue that need to be considered and closed in Rel-17) and based on that, determine whether to be included in the open issue list or not.

2nd phase: email discussion on the identified open issues with collecting companies’ inputs on the candidate options or rapporteur’s suggestion.

 **Intended outcome:** Open issue list with the proposed candidate options or rapporteur’s suggestion from 1st phase (in R2-2201806). Discussion summary for the identified open issues from 2nd phase.

**Deadline:** 1st phase (1/21 – 1/28 UTC), 2nd phase (2/9 – 2/14 UTC)

The discussion is focusing on the Phase-1 open issue list review according to the principle set by the Chairman’s in [1]. Since there has already been related initial discussions in [AT116b-e][704][V2X/SL] [2], the following discussions take the related conclusions, i.e. list of identified issues by Proposal 1 in [2], as the baseline.

**Contact list**

|  |  |  |
| --- | --- | --- |
| Company | Name | E-mail |
| OPPO | Bingxue Leng | lengbingxue@oppo.com |
|  |  |  |
|  |  |  |
|  |  |  |

# Review on open issue list for power-saving resource allocation

The Proposal 1 in [2] sets the scope of the RAN2 specific issues that need to be discussed for WI completion. In this section, the open issues for power-saving resource allocation are further specified at a more detailed level based on the scope set by [2]. Companies are invited to provide views on whether each issue is essential to be concluded in RAN2 #117-e and the suggested way of treatment/handling for each of them (i.e. Company input into Pre117-e-offline, Company tdocs invited, CR rapporteur handled issue, Other [1]).

## 2.1 Need of upper layer configuration for power saving resource allocation (Item “J” in P1 [2])

### [Issue 1] Should the resource allocation scheme(s) applicable in UE’s AS depend on the type of NR SL transmission configured by the upper layers? If yes, how such configuration should be reflected in the AS Spec (e.g. P2X vs. non-P2X as in LTE)?

**[Rapp’s remarks]** As explained in detail in [3], related procedures of LTE V2X SL transmission depend on “*if the UE is configured with P2X related or non-P2X related V2X sidelink communication*”, including resource pool configuration, resource pool selection and resource allocation scheme selection procedures (referencing 5.10.13.1, 5.10.13.1a and 5.10.13.2 in TS 36.331). If this LTE principle is followed, the specific type of NR SL communication configured by the upper layers, i.e. NR SL communication using power-saving resource allocation or not (or the said “power saved SL” in [4]), may be needed to control the resource allocation methods able to be used in AS. An alternative way may be no longer inheriting such upper layer configuration from LTE V2X SL, but depending on completely UE capability to decide the applicable resource allocation scheme(s) in UE’s AS. Basically, the issue is to check whether NR SL resource allocation scheme(s) are still subject to upper layer control (based on e.g. service type, authorization, etc.) as in LTE, or are now alternatively fully up to the AS itself to decide.

But regardless of whether way to go and in which Spec related procedures are captured, this issue needs to be concluded; otherwise RRC or MAC rapporteur cannot decide whether to specify the corresponding procedures based on upper layer configuration or directly based on UE AS capability.

**[Suggested WF] Issue 1 is an essential open issue that needs to be closed in RAN2 #117-e. Suggest to handle this issue based on “Company input into Pre117-e-offline”.**

**Companies’ views are invited on the suggested WF above for the handling of [Issue 1].**

|  |  |  |
| --- | --- | --- |
| **Company** | **Agree with the suggested WF? (Y/N)** | **Comments, if any (e.g. need of discussion, suggested way of handling, etc.)** |
| **OPPO** | **Y** |  |
|  |  |  |
|  |  |  |

**Companies are invited to provide initial inputs on the candidate options for [Issue 1] (if any).**

|  |  |  |
| --- | --- | --- |
| **Company** | **Candidate options (if any)** | **Justification on the options provided (if any)** |
| vivo | Option 1: Yes. A UE can be configured to perform NR SL transmission using power-saving resource allocation or NR SL transmission using non-power-saving resource allocation.Option 2: Yes. A UE can be configured to perform P2X related NR SL transmission or non-P2X related NR SL transmission (as in LTE). Option 3: No. A UE decides which resource allocation scheme can be used in the AS completely based on UE capability.  | Option 1 is based on the consideration that NR SL communication is not limit to the support of V2X services, so looks more comprehensive than Option 2.Option 3 is another way out, if companies in NR decide to no more rely on upper layer control of the applicable resource allocation schemes.  |
| OPPO | **No need for the upper layer configuration** on resource allocation, besides UE capability and resource pool configuration, leave it to UE implementation to select the resource allocation scheme. | Although we see issue 1 as an attempt to copy LTE, we are a bit reluctant since 1) **additional SA/CT work** cannot be avoided;2) according to our RAN1 colleagues, even **a VUE has power saving needs**, i.e., when the battery is low, which cannot be reflected by service type.Therefore, considering the **difference between LTE and NR**, in order to **accomplish the WI in time**, besides the resource pool configuration and UE capability agreed by RAN1, we prefer to leave it to UE implementation to decide the resource allocation schemes. |
|  |  |  |

## 2.2 Report of the type of NR SL transmission for RRC\_CONNECTED UE (Item “E” in P1 [2])

### [Issue 2]: Is there a case that an RRC\_CONNECTED UE needs to report the actual type of NR SL transmission it is configured to perform to the gNB (e.g. due to authorization allowing both power-saving and non-power saving resource allocation schemes)?

**[Rapp’s remarks]** As explained in detail in [3], this issue exists in LTE V2X SL communication when a UE is authorized as both a P-UE and a V-UE. Though such authorization information also exists in NR PC5 SA2 Spec TS 23.287, it is not clear whether it is of a similar use for NR SL communication as in LTE V2X SL. If a similar case holds in NR SL as well, an RRC\_CONNECTED UE may need to report the type of NR SL communication it is really configured to perform to the gNB, in order for the gNB to judge whether to provide resource configurations for power-saving resource allocation or those for non-power-saving resource allocation.

Note that this issue has also dependency on the conclusion of Issue 1: if in NR we alternatively depend on UE capability only to decide the applicable resource allocation scheme in the AS (i.e. out of control from upper layer authorization/configuration), the gNB can simply provide the resource configurations based on UE capability signalling on resource allocation schemes supported. With above situations, it is worth checking companies’ views on which way to go, and make a corresponding agreement to be reflected in the Spec.

**[Suggested WF] Issue 2 is an essential open issue that needs to be closed in RAN2 #117-e. Suggest to handle this issue based on “Company input into Pre117-e-offline”.**

**Companies’ views are invited on the above suggested WF for the handling of [Issue 2].**

|  |  |  |
| --- | --- | --- |
| **Company** | **Agree with the suggested WF? (Y/N)** | **Comments, if any (e.g. need of discussion, suggested way of handling, etc.)** |
| **OPPO** | **N to authorization part, Y to the report**  | **Firstly, we do not think the authorization is needed, which does not exist in LTE and everything works well, so it does not seem a critical issue on the table;****Secondly, we understand the source of the report considering LTE solution, although we are not in favour of upper layer configuration as commented in Issue 1;** |
|  |  |  |
|  |  |  |

**Companies are invited to provide initial inputs on candidate options for [Issue 2] (if any).**

|  |  |  |
| --- | --- | --- |
| **Company** | **Candidate options (if any)** | **Justification on the options provided (if any)** |
| vivo | Option 1: Yes, it reports whether it is configured to perform NR SL communication using power-saving or NR SL communication using non-power-saving resource allocation.Option 2: Yes, it reports whether it is configured to perform P2X or non-P2X NR SL communication (as in LTE).Option 3: No, RAN decides what resource allocation scheme to use based on UE capability only. | Options here need respectively correspond to the options for Issue 1. |
| OPPO | No need for UE report on SL communication type, NW can know based on UE capability. | we see this report is not needed **only if there is a UE type that is capable of both full-sensing and partial/random selection**, and in that case, **network implementation can work well** (by configuring resource pool(s) supporting all/any of the scheme(s) that UE is capable of) since NW already knows the UE capability. |
|  |  |  |

## 2.3 Resource pool configuration for power-saving resource allocation (Item “A” in P1 [2])

This issue was raided by several contributions, e.g. [3], [[4](file:///D%3A%5C3GPP%20RAN2%5CGeneral%5CRAN2%20%23116bise%5CTdoc%20Review%5CSL%20enh%5Csuccess%5CR2-2201591.docx)], [[5](file:///D%3A%5C3GPP%20RAN2%5CGeneral%5CRAN2%20%23116bise%5CTdoc%20Review%5CSL%20enh%5Csuccess%5CR2-2200317_Resource%20Allocation%20Enhancements.docx)], [[6](file:///D%3A%5C3GPP%20RAN2%5CGeneral%5CRAN2%20%23116bise%5CTdoc%20Review%5CSL%20enh%5Csuccess%5CR2-2200375-%20Discussion%20on%20resource%20allocation%20enhancement.docx)], [[7](file:///D%3A%5C3GPP%20RAN2%5CGeneral%5CRAN2%20%23116bise%5CTdoc%20Review%5CSL%20enh%5Csuccess%5CR2-2200379%20RAN2%20aspects%20on%20resource%20allocation%20enhancements%20for%20Rel-17%20eSL.docx)], [[8](file:///D%3A%5C3GPP%20RAN2%5CGeneral%5CRAN2%20%23116bise%5CTdoc%20Review%5CSL%20enh%5Csuccess%5CR2-2201457_RA-PowerReduction.docx)], [9]. There are three sub-level issues that need to be checked among companies: resource pool configuration IE, per-pool allowed resource allocation scheme configuration and CBPS vs. PBS configuration. Related issues are provided for companies’ review as follows.

### [Issue 3a] Is a separate pool configuration IE needed specifically for the power-saving resource allocation than the existing Rel-16 resource pool configuration IE?

### [Issue 3b] How should the per-pool allowed resource allocation scheme(s) be configured (which is related to the implementation of L1 RRC parameter *allowedResourceSelectionConfig*)?

**[Rapp’s remarks]** Issues 3a was mentioned by [[3](file:///D%3A%5C3GPP%20RAN2%5CGeneral%5CRAN2%20%23116bise%5CTdoc%20Review%5CSL%20enh%5Csuccess%5CR2-2200379%20RAN2%20aspects%20on%20resource%20allocation%20enhancements%20for%20Rel-17%20eSL.docx)], [[6](file:///D%3A%5C3GPP%20RAN2%5CGeneral%5CRAN2%20%23116bise%5CTdoc%20Review%5CSL%20enh%5Csuccess%5CR2-2200375-%20Discussion%20on%20resource%20allocation%20enhancement.docx)] and [[7](file:///D%3A%5C3GPP%20RAN2%5CGeneral%5CRAN2%20%23116bise%5CTdoc%20Review%5CSL%20enh%5Csuccess%5CR2-2201457_RA-PowerReduction.docx)]. Issue 3b was mentioned by [5], [[8](file:///D%3A%5C3GPP%20RAN2%5CGeneral%5CRAN2%20%23116bise%5CTdoc%20Review%5CSL%20enh%5Csuccess%5CR2-2200317_Resource%20Allocation%20Enhancements.docx)] and [9]. They are, however, having some coupling with each other. On the one hand, the field description of parameter *allowedResourceSelectionConfig* in RAN1 RRC parameter list [10] is “Indicates the allowed resource selection mechanism(s), i.e. full sensing only, partial sensing only, random resource selection only, or *any combination(s) thereof*”. If this “*… any combination(s) thereof*” is strictly followed in any case, there cannot be a separate power-saving specific resource pool configuration, as these pools do not allow full sensing to be configured. On the other hand, paper in [[6](file:///D%3A%5C3GPP%20RAN2%5CGeneral%5CRAN2%20%23116bise%5CTdoc%20Review%5CSL%20enh%5Csuccess%5CR2-2200375-%20Discussion%20on%20resource%20allocation%20enhancement.docx)] raised a valid point to avoid interference caused by Rel-16 full-sensing UEs to Rel-17 power-saving UEs in the legacy pool configurations. At least from signalling design point of view, RAN2 needs to have a conclusion on how such configuration aspect should be; otherwise, how to capture such per-pool configuration on allowed resource allocation schemes would be unclear.

**[Suggested WF] Issue 3a and Issue 3b are essential open issues that need to be closed in RAN2 #117-e. Suggest to handle them based on “Company input into Pre117-e-offline”.**

**Companies’ views are invited on the above suggested WF for the handling of [Issue 3a] and [Issue 3b].**

|  |  |  |
| --- | --- | --- |
| **Company** | **Agree with the suggested WF? (Y/N)** | **Comments if any** |
| **For issue 3a** | **For issue 3b** |
| **OPPO** | **Y** | **N** | **Our understanding is these 2 issues are already concluded by RAN1.****For issue 3a, we understand there could be different view, so OK to discuss it. Our understdning is according to RAN1 agreement/RRC parameter (allowedResourceSelectionConfig), the resource pool can be configured to support full sensing only; partial sensing only; random resource selection only; any combination(s) thereof. Which means a separate pool configuration IE is needed since the full sensing cannot be disabled in legacy(R16) resource pool, i.e., the partial sensing only, partial sensing+random selection pool cannot be supported W/O R17 specific resource pool;****For issue 3b, we think this is concluded by RAN1, and it is straightforward to implement the RRC parameter list as concluded by R1, so not sure what is to be discussed.****Therefore, we think we can follow RAN1 agreements directly.**  |
|  |  |  |  |
|  |  |  |  |

**Companies are invited to provide initial inputs on candidate options for [Issue 3a] and [Issue 3b] (if any).**

|  |  |  |  |
| --- | --- | --- | --- |
| **Company** | **Candidate options for Issue 3a (if any)** | **Candidate options for Issue 3b (if any)** | **Justification on the options provided (if any)** |
| vivo | Option 1: Yes, a separate pool configuration IE which is only visible to Rel-17 UEs is introduced for power saving resource allocation.Option 2: No, reuse existing Rel-16 pool configuration IE.  | Option 1: In the separate pool configuration specific for power saving resource allocation, “partial sensing only”, “random selection only” or “both” can be configured (as in LTE P2X).Option 2: In a pool, any combination among “partial sensing allowed”, “random sensing allowed” and full “sensing allowed” can be configured (totally 7 possible combinations). | Options for Issue 3b need respectively correspond to the options for Issue 3a. |
| OPPO | As replied in the above question, we think the separate resource pool is already a RAN1 conclusion. | As replied in the above question, we think it is already a RAN1 conclusion, there is no need to deviate from R1 RRC parameter list due to the discussion for 3a. |  |
|  |  |  |  |

### [Issue 3c] For a resource pool enabled with “partial sensing”, is it needed to further configure whether it is the CPS or PBPS or both that is enabled?

**[Rapp’s remarks]** This issue was raised by [[4](file:///D%3A%5C3GPP%20RAN2%5CGeneral%5CRAN2%20%23116bise%5CTdoc%20Review%5CSL%20enh%5Csuccess%5CR2-2201591.docx)]. RAN2 needs to reach common understanding based on RAN1’s progress, in order to decide whether any further signalling is needed.

**[Suggested WF] Issue 3c is an essential open issue that needs to be closed in RAN2 #117-e. Suggest to handle this issue based on “Company input into Pre117-e-offline”.**

**Companies’ views are invited on the above suggested WF for the handling of [Issue 3c].**

|  |  |  |
| --- | --- | --- |
| **Company** | **Agree with the suggested WF? (Y/N)** | **Comments, if any (e.g. need of discussion, suggested way of handling, etc.)** |
| **OPPO** | **N** | **Although we understand there might be a proposal behind 3c, we do not see it is a critical issue considering it goes against R1 conclusion, so should not be on the table for discussion here.****RAN1 has made clear conclusion on the condition of performing PBPS and CPS, we don’t think there is a need to introduce additional L2 condition/indication for differentiation of CPS and PBPS.** |
|  |  |  |
|  |  |  |

 **Companies are invited to provide initial inputs on candidate options for [Issue 3c] (if any).**

|  |  |  |
| --- | --- | --- |
| **Company** | **Candidate options (if any)** | **Justification on the options provided (if any)** |
| vivo | Option 1: Yes, new signalling is needed to differentiate CPS and PBPS in a per-pool manner.Option 2: No, RAN1 has not introduced a configuration parameter to make such differentiation in a pool. |  |
| OPPO | No need for differentiate CPS and PBPS in (resource pool) configuration, stick to R1 RRC parameter list. |  |
|  |  |  |

## 2.4 Resource pool selection and resource allocation scheme selection (Item “B” and “D” in P1 [2])

The issues on pool selection and resource application scheme selection were discussed in [[3](file:///D%3A%5C3GPP%20RAN2%5CGeneral%5CRAN2%20%23116bise%5CTdoc%20Review%5CSL%20enh%5Csuccess%5CR2-2200379%20RAN2%20aspects%20on%20resource%20allocation%20enhancements%20for%20Rel-17%20eSL.docx)], [[4](file:///D%3A%5C3GPP%20RAN2%5CGeneral%5CRAN2%20%23116bise%5CTdoc%20Review%5CSL%20enh%5Csuccess%5CR2-2201591.docx)], [[5](file:///D%3A%5C3GPP%20RAN2%5CGeneral%5CRAN2%20%23116bise%5CTdoc%20Review%5CSL%20enh%5Csuccess%5CR2-2200317_Resource%20Allocation%20Enhancements.docx)], [[6](file:///D%3A%5C3GPP%20RAN2%5CGeneral%5CRAN2%20%23116bise%5CTdoc%20Review%5CSL%20enh%5Csuccess%5CR2-2200375-%20Discussion%20on%20resource%20allocation%20enhancement.docx)] and [9]. RAN1 has no conclusion on these aspects, and thus RAN2 needs to conclude these issues. Actually, in LTE V2X SL and NR SL, pool selection and resource allocation scheme selection were all concluded by RAN2, and reflected in RAN2 Specs.

### [Issue 4a] Is it agreeable that as in LTE, it is up to UE implementation to select a TX resource pool by taking into account the pool-specific resource allocation scheme(s) configured?

### [Issue 4b] Is it agreeable that as in LTE, it is up to UE implementation to select the resource allocation scheme finally used in the selected resource pool (if the selected pool allows multiple resource allocation schemes the UE is configured/capable to perform)?

**[Rapp’s remarks]** The two issues are coupled, as when the UE is configured with multiple mode-2 transmission pools, the UE needs to first select a resource pool, and in the selected pool, further selects the resource allocation scheme to be eventually used, if the selected pool allows more than one resource allocation schemes. Considering the limited time left, the issues are formulated to directly check companies’ views on whether the implemented-specific method as in LTE V2X SL can be reused. No matter whether finally the implementation-specific way is concluded or not, there needs to be related agreements on these issues, so as for the running CR rapporteurs (RRC or MAC) to reflect them in the corresponding Spec in a proper way. Note that the “configured/capable to perform” in above Issue 4b depends on the outcome of Issue 1 regarding whether an upper layer configuration is needed.

**[Suggested WF] Issue 4a and Issue 4b are essential open issues that need to be closed in RAN2 #117-e. Suggest to handle them based on “Company input into Pre117-e-offline”.**

**Companies’ views are invited on the suggested WF for the handling of [Issue 4a] and [Issue 4b].**

|  |  |  |
| --- | --- | --- |
| **Company** | **Agree with the Suggested WF (Y/N)** | **Comments, if any (e.g. need of discussion, suggested way of handling, etc.)** |
| **For issue 4a** | **For issue 4b** |
| **OPPO** | **N** | **Y** | **We understand in LTE, the resource allocation scheme is not an input to pool selection, while only zone and sync source is the input for pool selection. So do not see 4a as an critical issue to solve at the current stage.** |
|  |  |  |  |
|  |  |  |  |

**Companies are invited to provide initial inputs on candidate options for [Issue 4a] and [Issue 4b] (if any).**

|  |  |  |  |
| --- | --- | --- | --- |
| **Company** | **Candidate options for Issue 4a (if any)** | **Candidate options for Issue 4b (if any)** | **Justification on the options provided (if any)** |
| vivo | Option 1: Yes, no normative UE behaviour is needed.Option 2: No, it needs to be specified that a UE can only select a pool that includes at least one of the resource allocation schemes it is capable/configured to perform.  |  |  |
| OPPO | we do not see the need to have resource allocation scheme based pool selection.  | Yes, no normative UE behaviour is needed. |  |
|  |  |  |  |

## 2.5 Resource allocation scheme in the exceptional pool (Item “G” in P2 [X])

### [Issue 5] Is it agreeable that a UE only uses random resource selection in the exceptional pool?

**[Rapp’s remarks]** RAN1 did not conclude whether those power-saving resource allocation schemes apply to exceptional pool or not. In fact, nearly all exception pool handling has been concluded by RAN2 in both LTE V2X SL or NR SL. Therefore, RAN2 needs to make a decision.

**[Suggested WF] Issue 5 is an essential open issue that needs to be closed in RAN2 #117-e. Suggest to handle it based on “Company input into Pre117-e-offline”.**

**Companies’ views are invited on the above suggested WF for the handling of [Issue 5].**

|  |  |  |
| --- | --- | --- |
| **Company** | **Agree with the suggested WF? (Y/N)** | **Comments, if any (e.g. need of discussion, suggested way of handling, etc.)** |
| **OPPO** | **N** | **We fail to understand why this is an issue.** |
|  |  |  |
|  |  |  |

 **Companies are invited to provide initial inputs on candidate options for [Issue 5] (if any).**

|  |  |  |
| --- | --- | --- |
| **Company** | **Candidate option (if any)** | **Justification on the options provided (if any)** |
|  |  |  |
|  |  |  |
|  |  |  |

## 2.6 Re-evaluation/Pre-emption in partial sensing case (Item “H” in P1 [2])

### [Issue 6] Are there any RAN1-led impacts to MAC spec on the re-evaluation and pre-emption related procedure for partial sensing?

**[Rapp’s remarks]** The issue comes from contribution [8]. However, it actually only proposes that re-evaluation and pre-emption should apply for partial sensing as well. Rapporteur understands that till now there is no RAN1/2 conclusion to prohibit re-evaluation and pre-emption from being used for partial sensing. On the other hand, re-evaluation and pre-emption are both RAN1 designed features, and in Rel-16 the related procedures in the MAC were captured completely based on RAN1 agreements w/o any functional discussion in RAN2. Even if there is any impact that needs to be done to the MAC for partial sensing case, that should come from RAN1 agreements. RAN2 is unlikely to carry out any functional discussions for this feature. To this end, rapporteur thinks that the issue can be directly handled in the MAC running CR discussion regarding how to capture related RAN1 agreements (if really any).

**[Suggested WF] Issue 6 depends on whether any MAC Spec is needed based on the latest RAN1 progress. Suggest to handle it as a “CR rapporteur handled issue” during running CR discussion.**

**Companies’ views are invited on the above suggested WF for the handling of [Issue 6].**

|  |  |  |
| --- | --- | --- |
| **Company** | **Agree with the suggested WF? (Y/N)** | **Comments, if any (e.g. need of discussion, suggested way of handling, etc.)** |
| **OPPO** | **N** | **We did not see R1 attempt in this direction, so do not think this is a critical issue to solve now.** |
|  |  |  |
|  |  |  |

## 2.7 CBR related (Item “F” in P1 [2])

### [Issue 7a] Is it common understanding that CBR measurement is NOT supported, when the UE is performing random resource selection?

**[Rapp’s remarks]** This simply impacts whether/how to add a restriction in the CBR measurement procedure in RRC to exclude UEs performing random selection. In LTE, there is a similar restriction to exclude P2X related V2X SL communication for CBR measurement (i.e. “The UE capable of CBR measurement when configured to transmit **non-P2X** related V2X sidelink communication shall:” in 5.5.3.1, TS 36.331). There was a RAN1 agreement in RAN1 #107e that “When UE performs random resource selection, LTE principle is reused:”. So intuitively, a similar restriction needs to apply to the UE performing random selection in NR SL. Note that the difference in NR SL is that unlike P2X in LTE, UE performing partial sensing may still need to perform CBR. Considering the already clear RAN1 agreement to reuse LTE principle, this issue can be treated as an open issue in the running CR discussion.

**[Suggested WF] Issue 7a depends on whether any RRC Spec is needed based on the latest RAN1 progress. Suggest to handle it as a “CR rapporteur handled issue” during running CR discussion.**

**Companies’ views are invited on the above suggested WF for the handling of [Issue 7a]**

|  |  |  |
| --- | --- | --- |
| **Company** | **Agree with the suggested WF? (Y/N)** | **Comments, if any (e.g. need of discussion, suggested way of handling, etc.)** |
| **OPPO** | **Y** |  |
|  |  |  |
|  |  |  |

### [Issue 7b] Whether to reuse the existing parameter *sl-DefaultTxConfigIndex* or introduce a new parameter, whenever a (pre-)configured SL CBR is needed for partial sensing and random selection as per RAN1 agreements?

**[Rapp’s remarks]** There were several RAN1 agreements for both partial sensing and random selection, mentioning that “When no SL CBR measurement result is available, a (pre-)configured SL CBR value is used”. Also, in RAN1 #107b-e, there was a further RAN1 agreement for partial sensing that “If the number of SL RSSI measurement slots is below a (pre-)configured threshold, a (pre-)configured SL CBR value is used”. For partial sensing and random selection, one main use of the CBR value is to determine the parameters used for “CBR-priority” based link adaptation, and there has already been a (pre-)configured parameter set, i.e. via *sl-DefaultTxConfigIndex*, in the current RRC Spec to cope with this “no SL CBR available” case. Companies’ understanding needs to be checked on whether this existing parameter is already sufficient from a functional point of view based on related RAN agreements, so to decide whether to introduce a new parameter or not.

**[Suggested WF] Issue 7b is an essential open issue that needs to be closed in RAN2 #117-e. Suggest to handle it based on “Company input into Pre117-e-offline”.**

**Companies’ views are invited on the above suggested WF for the handling of [Issue 7b].**

|  |  |  |
| --- | --- | --- |
| **Company** | **Agree with the suggested WF? (Y/N)** | **Comments, if any (e.g. need of discussion, suggested way of handling, etc.)** |
| **OPPO** | **N** | **We tend to believe this issue can be fully rely on R1 conclusion, not see the space for R2 discussion yet.** |
|  |  |  |
|  |  |  |

**Companies are invited to provide initial inputs on candidate options for [Issue 7b] (if any).**

|  |  |  |
| --- | --- | --- |
| **Company** | **Candidate options (if any)** | **Justification on the options provided (if any)** |
|  |  |  |
|  |  |  |
|  |  |  |

## 2.8 RAN2 impact on partial sensing due to SL DRX (Item “C” and “I” in P1 [2])

**[Rapp’s remarks]** Contributions discussing SL-DRX impacts on partial sensing mainly include references in [[6](file:///D%3A%5C3GPP%20RAN2%5CGeneral%5CRAN2%20%23116bise%5CTdoc%20Review%5CSL%20enh%5Csuccess%5CR2-2200375-%20Discussion%20on%20resource%20allocation%20enhancement.docx)], [[7](file:///D%3A%5C3GPP%20RAN2%5CGeneral%5CRAN2%20%23116bise%5CTdoc%20Review%5CSL%20enh%5Csuccess%5CR2-2201457_RA-PowerReduction.docx)], [11] and [[12](file:///D%3A%5C3GPP%20RAN2%5CGeneral%5CRAN2%20%23116bise%5CTdoc%20Review%5CSL%20enh%5Csuccess%5CR2-2201479%20-%20Interaction%20between%20partial%20sensing%20and%20DRX.docx)]. One of the issues raised by [[11](file:///D%3A%5C3GPP%20RAN2%5CGeneral%5CRAN2%20%23116bise%5CTdoc%20Review%5CSL%20enh%5Csuccess%5CR2-2201479%20-%20Interaction%20between%20partial%20sensing%20and%20DRX.docx)] and [12] is to confirm partial sensing is only performed by the UE during SL DRX active time. In fact, RAN1 already reached final conclusions on how UE performs partial sensing when SL DRX is configured in RAN1 #107b-e, and since sensing is a pure RAN1 functionality, with already RAN1 conclusions, RAN2 does not need to further make any conclusion on this issue. The other issue raised by all above contributions is about whether to support SL DRX configuration and PBPS configuration alignment, with the contributions in [7] and [[11](file:///D%3A%5C3GPP%20RAN2%5CGeneral%5CRAN2%20%23116bise%5CTdoc%20Review%5CSL%20enh%5Csuccess%5CR2-2201457_RA-PowerReduction.docx)] proposing such enhancements but the contribution in [[6](file:///D%3A%5C3GPP%20RAN2%5CGeneral%5CRAN2%20%23116bise%5CTdoc%20Review%5CSL%20enh%5Csuccess%5CR2-2200375-%20Discussion%20on%20resource%20allocation%20enhancement.docx)] and [[12](file:///D%3A%5C3GPP%20RAN2%5CGeneral%5CRAN2%20%23116bise%5CTdoc%20Review%5CSL%20enh%5Csuccess%5CR2-2201479%20-%20Interaction%20between%20partial%20sensing%20and%20DRX.docx)] indicating no need for it as an optimization. As sensing operation is a RAN1 feature and RAN1 did not conclude the necessity to introduce such a configuration alignment, it means that this feature is not essential from RAN1 perspective. Therefore, such an alignment should be regarded as optimizations in RAN2 as well.

Based on above survey on companies’ contributions, rapporteur understands that there may not be essential open issues that need to be discussed in RAN2 for this SL DRX impact on power-saving resource allocation. Also note that the *general* SL DRX impacts on resource allocation (instead of power-saving resource allocation specific aspects, e.g. LCP impact) have always been handled in SL DRX AI. This should be followed in the next meeting as well.

**[Suggested WF] No essential open issue from RAN2 perspective needs to be closed in RAN2 #117-e for SL-DRX impacts on power-saving resource allocation.**

**Companies’ views are invited on the above suggested WF for the handling of SL DRX impact on power-saving resource allocation**

|  |  |  |
| --- | --- | --- |
| **Company** | **Agree with the suggested WF? (Y/N)** | **Comments, if any (e.g. need of discussion, suggested way of handling, etc.)** |
| **OPPO** | **Y** |  |
|  |  |  |
|  |  |  |

## 2.9 Others

**Any essential RAN2 open issue is missing? Please provide input to the following table, if any.**

|  |  |
| --- | --- |
| **Company** | **Other critical RAN2 open issues identified (if any)** |
|  |  |
|  |  |
|  |  |

# Output Open Issue List and Recommendations

# References

1. R2-22xxxxx Coordinated Company Input For Rel-17 Open Issues Planning R2 117-e and impacts to R2 116bis-e RAN2 Chair
2. R2-2201804 Summary [AT116b-e][704][V2X/SL] Resource allocation enhancements LG Electronics Inc. (Rapporteur)
3. R2-2200379 RAN2 aspects on resource allocation enhancements for Rel-17 eSL vivo
4. R2-2201591 Resource allocation enhancements Samsung
5. R2-2200317 Consideration on Resource Allocation Enhancements CATT
6. R2-2200375 Discussion on resource allocation enhancement OPPO
7. R2-2201457 Power Reduction for Sidelink Mode 2 Resource Allocation Fraunhofer IIS, Fraunhofer HHI
8. R2-2200529 On resource allocation and inter-UE coordination Intel Corporation
9. R2-2110940 Resource pool configuration and selection of resource selection mechanism Samsung
10. R1-2112976 Consolidated higher layers parameter list for Rel-17 NR
11. R2-2107629 NR SL Resource allocations for Pedestrian UEs Apple
12. R2-2201479 Interaction between partial sensing and DRX Ericsson