**3GPP T****SG-RAN WG2 Meeting #123 R2-230xxxx**

Toulouse, France, 21- 25August, 2023

Agenda Item: 7.13.2

Source: CMCC (moderator)

Title: Summary of [Post122][584][R18 SON/MDT] Open issues on fast MCG recovery

Document for: Discussion and Decision

# Introduction

This document is the report of the following email discussion,

* **[Post122][584][R18 SON/MDT] Open issues on fast MCG recovery (CMCC)**

Scope: Discussion should focus on the proposals raised and not concluded in R2-2305779.

Intended outcome: Report

 Deadline: Long

Please provide your comments before Aug. 09th, 23:59 UTC

# Contact Information

Participants are encouraged to leave their contact information in the following table.

|  |  |
| --- | --- |
| Company | Contact info (name, email address) |
|  CMCC |  Fang Xie, xiefang@chinamobile.com |
|  CATT | Haocheng Wang, wanghaocheng@catt.cn |
|  Samsung | Aby K Abraham aby.abraham@samsung.com |
|   |   |
|   |   |
|   |   |

# Discussion

In RAN2#122 meeting, companies agreed to introduce the near failure case for fast MCG recovery and initial agreements on fast MCG recovery are concluded as follows:

Agreements:

1 RAN2 confirms scenario of near failure fast MCG recovery.

2 RAN2 confirms scenario f1, i.e., SCG fails or is deactivated before the UE sends the MCGFailureInformation. FFS RAN2 impact.

In this email discussion, the open issues on fast MCG recovery are mainly based on the proposals provided in R2-2305779, including the information for the optimization of near failure of fast MCG recovery reported by UE, T316 related triggering threshold and time information reported by UE for fast MCG link recovery optimization.

## Information reported by UE for the optimization of near failure of fast MCG recovery

Following options are proposed in R2-2305779 for UE to report for the optimization of near failure of fast MCG recovery:

Option 1: Elapsed T316 between the transmission of MCGFailureInformation and receiving RRC reconfiguration or RRC release message;

Option 2: The ratio between the elapsed T316 and the configured value of T316;

**Question 1: Companies are invited to provide the views on which information should be reported by UE for the optimization of near failure of fast MCG recovery.**

|  |  |
| --- | --- |
| **Company** | **Comments** |
| CMCC | From our view, both options can help network to detect potential underlying issues and optimize the configuration of T316. Option 1 is preferred, since for option 2 the network needs to remember the configured T316.  |
| CATT | Either is OK to us. |
| Samsung | Option 1 seems to be simpler. |
|  |  |

## T316 related triggering threshold

In R2-2305779, it is proposed that UE could only report the information when a triggering threshold is met, e.g., T316 exceeds a configured threshold, to reduce the unnecessary reporting for fast MCG link recovery near failure case, which is similar to SNR.

**Question 2: Companies are invited to provide the views on whether to introduce the T316 related triggering threshold.**

|  |  |
| --- | --- |
| **Company** | **Comments** |
| CMCC | We support to introduce the T316 related triggering threshold. Only if the triggering threshold is met, UE generates and reports the information, which will reduce the reporting overhead for UE. |
| CATT | Agree with CMCC, and maybe the similar thresholds configuration of SHR T310 can be reused: ENUMERATED {p40, p60, p80, spare5, spare4, spare3, spare2, spare1}. |
| Samsung | We do not support introducing the T316 related trigger. We think that the overhead for reporting the information is not very high irrespective of the option 1/ option 2 chosen in 3.1. It is 6 bits/ 11 bits of information and the UE can easily include this information in the existing RLF report. On the other hand, if we keep adding new thresholds for each information, the UE and network implementation will become much complex.  |
|  |  |

## Time information reported by UE for fast MCG link recovery optimization

Until now, following cases for fast MCG link recovery have been agreed to be addressed in both RAN2 and RAN3:

* Case a: SCG fails when the UE is undergoing fast MCG recovery (i.e. SCG failure happens while T316 is running)
* Case f1: SCG fails or is deactivated yet before the UE sends the MCGFailureInformation
* Case b: the signalling delay is longer than the time the UE waits for the response (T316 expired)

Regard to fast MCG link recovery optimization, some time-related information is also beneficial for network to understand the situation of SCG and do further optimization of fast MCG recovery, e.g., the time between MCG failure (or transmitting MCGFailureInformation) and SCG failure or SCG deactivation.

Therefore, for case a, UE reports the time between MCG failure (or transmitting MCGFailureInformation) and SCG failure. For case f1, UE reports the time between MCG failure (or transmitting MCGFailureInformation) and SCG failure or SCG deactivation.

**Question 3:** **Companies are invited to provide the views on whether to agree to report the time information for fast MCG link recovery optimization in the proposal listed below.**

**Proposal: UE reports following time information for fast MCG link recovery optimization:**

* **Time between MCG failure (or transmitting MCGFailureInformation) and SCG failure for case a and f1**
* **Time between MCG failure (or transmitting MCGFailureInformation) and SCG deactivation for case f1**

|  |  |
| --- | --- |
| **Company** | **Comments** |
| CMCC | We support to report the above time information for fast MCG link recovery optimization. For the scenario that both MCG failure and SCG failure happen in a short time, it means there is a coverage issue, since the UE cannot connect to the network at all, the coverage enhancement is necessary. For the scenario that both MCG failure and SCG deactivation happen in a short time, it means the decision of SCG deactivation is not appropriate, so the principle to deactivate SCG needs further optimization. |
| CATT | Agree with CMCC, at least the time between MCG failure and SCG failure should be introduced since the time can be used to indicate whether the coverage problem of the MN an SN maybe occurred in a nearby location. Then some optimization can be performed.For the MCG failure and SCG deactivation scenario, the NW could consider reducing the possibility of initiating SCG deactivation near the location of MCG failure, so that MCG link can be recovery as much as possible. |
| Samsung | Until now, following cases for fast MCG link recovery have been agreed to be addressed in both RAN2 and RAN3:* Case a: SCG fails when the UE is undergoing fast MCG recovery (i.e. SCG failure happens while T316 is running)
* Case f1: SCG fails or is deactivated yet before the UE sends the MCGFailureInformation
* Case b: the signalling delay is longer than the time the UE waits for the response (T316 expired)

For simplicity, we suggest to include the indications to identify why MCG failure information procedure was not initiated, rather than the time information. * Indication to indicate if T316 is configured
* Indication to indicate if SCG transmission is not suspended
* Indication to indicate if the SCG is not deactivated
* Indication to indicate if neither PSCell change nor PSCell addition is ongoing
* Indication to indicate whether SRB2 and at least one DRB or multicast MRB setup.

This is aligned with the agreements from RAN2/RAN3 (such as RAN3 agreement “log SCG was deactivated or other cases that SCG is not available” and RAN2 agreement “Fast MCG recovery failure cause shall be included for fast MCG recovery optimization”).If the UE is not able to initiate MCG Failure Information procedure due to SCG failure (case f1), the SCG failure would have occurred in a very less time before the MCG failure as otherwise MN would have restored SCG. This means that network can identify there is a SCG coverage issue before a very short period (usually in the order of milliseconds) before MCG failure, and this is enough for the optimization. Benefits of reporting actual time is questionable.Similarly SCG deactivation and MCG failure occurring together (case f1) is also a corner case. SCG deactivation is based normally on the amount of data in SCG bearers, and not coverage. Hence the indication is enough and time is not much helpful.For case a, if the UE stores the elapsed timer for T316 as in 3.1 and the SCG failure type as already agreed in RAN3, time information is not needed. Elapsed timer of T316 gives the time between initiating the fast MCG link recovery and the SCG Failure. |
|  |  |

## In which report to capture fast MCG recovery related information

As for in which report to capture fast MCG recovery related information, we would like to ask the following question.

**Question 4: Companies are invited to provide their view on which report to be used for supporting data collection for above information.**

1. **Existing RLF report**
2. **SHR**
3. **New report**

|  |  |  |
| --- | --- | --- |
| **Company** | **(A/B/C)** | **Comments** |
| CMCC | A | Since the UE will generate an RLF report when MCG failure occurs, it is straightforward to reuse it to collect fast MCG recovery related information. |
| CATT | A for failure;B for near failure | RLF report is appropriate to include all the real failure scenario(s), but we think the near failure case (case c) can reuse the SHR mechanism since the triggering threshold should be configured by the NW. |
| Samsung | A | Agree with CMCC. We already agreed that RLF report is enhanced to support fast MCG recovery MRO in RAN2#120.  |
|  |  |  |

# Conclusion

If needed.

# Reference

1. R2-2305779, Further considerations on fast MCG recovery, CMCC