|  |  |  |  |
| --- | --- | --- | --- |
| Company | Clause | Comment | Rapp Response |
| Xiaomi | 6.3.5 | Field description of sl-LBT-FailureRecoveryConfig  Configures parameters used for detection of sidelink consistent ~~sidelink~~ LBT failures for operation with shared spectrum channel access, as specified in TS 38.321 [3] |  |
| Xiaomi | 6.3.5 | FD of sl-FreqInfoToAddModListExt is added to sl-FreqInfoToReleaseList  Seems typo should be added after sl-FreqInfoToAddModList |  |
| Xiaomi | 6.3.5 | FD of sl-FreqInfoToAddModList should clarify that  In this release, only one entry can be configured in sl-FreqInfoToAddModList  The sentence still applies to sl-FreqInfoToAddModList  Can not be directly deleted. |  |
| Xiaomi | 6.3.5 | sl-FreqInfoToReleaseList  Do we need sl-FreqInfoToReleaseListExt? |  |
| Xiaomi | 6.3.5 | FD of sl-RLC-BearerToReleaseList, sl-RLC-BearerToReleaseListSizeExt  Should have similar sentence that “The UE shall consider entries in sl-RLC-BearerToReleaseList and sl-RLC-BearerToReleaseListSizeExt as a single list, i.e. an entry created using sl-RLC-BearerToAddModList and in sl-RLC-BearerToAddModListSizeExt  can be deleted using sl-RLC-BearerToReleaseList or sl-RLC-BearerToReleaseListSizeExt |  |
| Xiaomi | 6.3.5 | sl-PDCP-config  we need to have indication to enable PDCP duplication?  moreThanOneRLC SEQUENCE {  primaryPath SEQUENCE {  cellGroup CellGroupId OPTIONAL, -- Need R  logicalChannel LogicalChannelIdentity OPTIONAL -- Need R  },  ul-DataSplitThreshold UL-DataSplitThreshold OPTIONAL, -- Cond SplitBearer  pdcp-Duplication BOOLEAN OPTIONAL -- Need R  } OPTIONAL, -- Cond MoreThanOneRLC |  |