|  |  |  |  |
| --- | --- | --- | --- |
| Company | Clause | Comment | Rapp Response |
| Apple | 16.9.Y | Issue:  " Carrier (re)selection may be performed and a new carrier configuration is reported to the RX UE when the TX UE detects carrier failure on a specific carrier, as specified in 3GPP TS 38.321 [x]."  It is not clear what "a new carrier configuration is reported to the RX UE" means, and we generally don't say a configured is reported.  Solution:  According to below agreement in last RAN2 meeting:  **Agreements on SL RLF**   1. In TX UE, per carrier “carrier failure” is introduced. If “carrier failure” is declared for a carrier, the carrier should be removed/released. The carrier (re)selection can be triggered. For UC, this carrier can be released via PC5 RRC reconfiguration.   We suggest below change:  " When the TX UE detects carrier failure on a specific carrier, carrier (re)selection may be performed and the concerned carrier can be released via PC5 RRC reconfiguration, as specified in 3GPP TS 38.321 [x]." |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |