3GPP TSG-RAN WG2 Meeting #124 R2-231xxxx

Chicago, USA, 13 – 17 November 2023

**Agenda item: 7.4.5**

**Source: Nokia (Rapporteur)**

**Title: [Post123bis][551][feMob] eEMR SCell setup delay (Nokia)**

**WID/SID: NR\_Mob\_enh2-Core - Release 18**

**Document for: Discussion and Decision**

# 1 Introduction

This document is the report of the following email discussion:

* [Post123bis][551][feMob] eEMR SCell setup delay (Nokia)

 Scope: Initial Identification of R2 impact and attempting RRC Draft CR (as far as reasonable given R4 progress). Due to short time between meetings – limited ambition level (only one round of comments).

 Intended outcome: Report, draft CR (that can be a baseline)

 Deadline: Long

# 2 Contact Points

Respondents to the email discussion are kindly asked to fill in the following table.

|  |  |  |
| --- | --- | --- |
| Company | Name | Email Address |
| Nokia (Rapporteur) | Jarkko Koskela | jarkko.t.koskela@nokia.com |
| CMCC | Xiaoman Liu | liuxiaoman@chinamobile.com |
| Ericsson | Cecilia Eklöf | cecilia.eklof@ericsson.com |
| Apple | Naveen Palle | naveen.palle@apple.com |
| CATT | Rui Zhou | zhourui@catt.cn |
| ZTE | Mengjie Zhang | zhang.mengjie@zte.com.cn |
| Huawei, HiSilicon | David Lecompte | david.lecompte@huawei.com |
| Xiaomi | Yi Xiong | xiongyi3@xiaomi.com |
| LGE | SungHoon Jung | sunghoon.jung@lge.com |
| MediaTek | Felix Tsai | Chun-fan.tsai@mediatek.com |
| Qualcomm | Punyaslok Purkayastha | punyaslo@qti.qualcomm.com |
| vivo | Wenjuan Pu | wenjuan.pu@vivo.com |
| OPPO | Xue Lin | linxue@oppo.com |
|  |  |  |

# 3 Background

RAN4 #106 agreed that UE is allowed to perform addition measurement starting from RRC connection setup/resume procedure. The overall solution with re-evaluation measurements is in our view as shown in Figure 1.



Figure 1: Timeline of the overall solution.

1. The overall solution consists of:

1. UE having measurements available from IDLE/INACTIVE mode at RRC setup/resume,
2. UE evaluates the validity of the available measurements during RRC connection setup/resume,
3. UE indicating the measurement status to the network at RRC setup/resume complete,
4. When needed for measurement validation purposes, UE continuing to perform measurements during the RRC setup/resume and the connected mode until reporting,
5. UE reporting the measurements results as soon as measurements have been completed.

 RAN4 provided a LS on this topic in R4-2314466 listing their agreements:

*RAN4 has been working on WID objective 7 on NR mobility enhancements, which (as per* [*RP-231475*](https://www.3gpp.org/ftp/meetings_3gpp_sync/ran/Docs/RP-231475.zip)*) is defined as per the following*

|  |
| --- |
| 1. *To study and specify how to reuse the IDLE/INACTIVE mode measurement results which are to be reported during and/or after RRC connection setup/resume in order to improve SCell/SCG setup delay [RAN4, RAN2], including:*
	* *Availability and validation of the IDLE/INACTIVE mode measurement results to be reported [RAN4]; and*
	* *Definition of corresponding RRM requirements [RAN4]; and*
	* *If necessary based on RAN4 outcome, definition of corresponding signalling support [RAN2].*

*Note 6: RAN4 will coordinate in due course with RAN2 to start the work.**Note 7: R4-2220415 serves as baseline for future work in RAN4**Note 8: With exception of the above scenarios, enhancements on IDLE/INACTIVE mode measurements and on UE behavior in IDLE/INACTIVE mode are not in scope.* |

*As the objective states, RAN4 aims to improve the availability of UE measurements to allow for faster FR2 SCG/SCell setup, starting from RRC connection setup/resume. RAN2 is kindly requested to define the corresponding signalling support based on the following RAN4 input:*

|  |
| --- |
| ***RAN4 #108 Agreements:*** *Measurement reporting****<Agreement>**** *For UE which is not capable of EMR, when the measurement results during idle/inactive mode are available and valid, UE can report these results to the network during or after RRC setup or resume procedures. The reporting procedure is up to RAN2.*

***<Agreement>*** * *It is up to UE implementation how to select a band to report unless NW specify a band to report.*

*Starting point of the enhanced measurement****<Agreement>**** *For MT originating call, UE starts to perform additional measurement after paging reception.*
* *And* *for MO call, UE starts to perform additional measurement after first RACH preamble transmission, i.e. Msg1.*
* *Note: the respective agreement can be used to derive requirements once feasibility of enhanced solution is confirmed*

*Ending point of the enhanced measurement****<Agreement>**** *The ending point of enhanced measurement at the reception of the RRC CONNECTED mode measurement configuration (the 1st RRC\_reconfiguration message)*
* *Note: the respective agreement can be used to derive requirements once feasibility of enhanced solution is confirmed*
 |

|  |
| --- |
| ***RAN4 #107: R4-2310064**** *Agreements:*
	+ *In new reporting in R18, UE does not report the invalid results to NW.*
 |

*RAN4 agreed general scope and common requirement as follow:*

|  |
| --- |
| ***RAN4 #106: R4-2303176******<Agreement>**** *RAN4 shall focus on inter-band target cell in FR2. If final solution to be agreed can cover intra-band and FR1 without extra standardization effort, it is unnecessary to exclude these two scenarios.*
* *UE is allowed to reuse existing measurement, including legacy measurement for cell re-selection and EMR.*
* *UE is allowed to perform addition measurement starting from RRC connection setup/resume procedure.*

***RAN4 #104-e R4-2214348******< Agreement>:*** * *DRX is not in use during RRC connection setup/resume procedure for enhanced measurement.*
 |

*RAN4 has discussed parallelly two solutions including solution based on existing measurement and solution based on enhanced measurement and has made the following latest agreements.*

1. *Solution based on existing measurement.*
2. *Solution based on enhanced measurement.*

 *RAN4 agreed that both solutions are not mutually exclusive.*

|  |
| --- |
| ***RAN4 #106-bis-e: R4-2306396******<Agreement>:**** *Solution based on existing measurement and solution based on enhanced measurement are not mutual exclusive. The two solutions are be discussed in parallel.*

***RAN4 #104-e R4-2214348*** ***<Agreement>:**** *Reduce the number of EMR carriers to be measured for improved measurement.*
* *FFS: how to select the frequency layers for improved measurement, how many frequency layers to measure and which scenario that is applicable.*
 |

*RAN4 is discussing whether new indication is needed and RAN4 is discussing conditions and UE behaviour performing additional measurement starting from RRC setup/resume.*

|  |
| --- |
| ***RAN4 #106-bis-e: R4-2306396******<Agreement>:****FFS : whether to introduce indication of availability and/or validity status of measurement results from UE to NW into the [existing] EMR reports.****RAN4 #106: R4-2303176******<Agreement>****RAN4 can continue discussion on the feasibility of doing additional measurement starting from RRC setup/resume, and requirements shall be defined if feasible solution is agreed.* |

RAN2 then made agreements in RAN2#123bis:

[R2-2310796](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_123bis/Docs/R2-2310796.zip) eEMR SCell setup delay Nokia, Nokia Shanghai Bell discussion Rel-18 NR\_Mob\_enh2-Core

- Nokia think most from existing EMR can be reused, but not the timer, as the measurements are expected to be started at connection setup.

- Nokia think we can start to work on the RRC CR.

- Ericsson think we can start on the CR and can reuse.

- MTK think this contains a lot of FFS, not sure it is useful to start CR discussion. Can identify R2 impact.

- QC think we cannot really capture anything, based on R4 progress. If R4 progress, we can do something.

- LGE think we can start some work .. but not CR. LGE think measurement configuration is different to EMR.

- Chair think R2 impact is limited, if R4 can conclude it should be possible to have CRs in R2.

* R2 expect to reuse legacy EMR to great extent
* Long email disc to next meeting, identifying R2 impact and attempting RRC Draft CR (Nokia)
* [Post123bis][551][feMob] eEMR SCell setup delay (Nokia)

 Scope: Identify R2 impact and attempting RRC Draft CR (as far as possible / reasonable given R4 progress)

 Intended outcome: Report, draft CR (that can be a baseline)

 Deadline: Next meeting

Additionally RAN4 made further agreements in RAN4#108bis (i.e. same time we had RAN2#123bis) which they informed in incoming LS (R4-2317428). NOTE: This has not been treated in RAN2 yet!:

|  |
| --- |
| **RAN4 #108bis** <Agreement>: * The measurements are considered valid if both of the following conditions are satisfied
	+ A) the measurement are performed within the last [X] seconds before it is reported
		- X value is network configured. Signalling details are up to RAN2
		- FFS on the X value(s) and will be decided by RAN4
		- If X is not defined then no requirements will be introduced
	+ B) the reported measurement results satisfy measurement accuracy [at the measurement instance]
	+ FFS on side conditions
 |

# 4 Discussion

So aim of email discuscsion is to continue:

* R2 expect to reuse legacy EMR to great extent
* Long email disc to next meeting, identifying R2 impact and attempting RRC Draft CR (Nokia)
* [Post123bis][551][feMob] eEMR SCell setup delay (Nokia)

 Scope: Identify R2 impact and attempting RRC Draft CR (as far as possible / reasonable given R4 progress)

 Intended outcome: Report, draft CR (that can be a baseline)

 Deadline: Next meeting

Even though legacy (R16) EMR is taken as baseline for working on the CRs there are some notable differences that need to be considered.

## 4.1 How to configure what to measure

For R16 Idle/Inactive measurement configuration is given in *RRCRelease* in *measeIdleConfig-r16.* It seems logical to add in that configuration new r18 part that involves FR2 carriers. Although RAN4 LS talks about “configuring band” in RAN2 we configure a carrier (ARFCN). From rapporteur point of view this seems to be just band terminology choice by RAN4.

**Question 1**: Should we configure ARFCN of the enhanced measurements target instead of band (i.e. like basically always done currently for any measurements)?

|  |
| --- |
| Answers to Question 1 |
| Company | Yes/No | Technical Arguments |
| CMCC | Yes |  The current way in the spec can be reused. |
| Ericsson |  | The current configuration in MeasIdleCarrierNR-r16 can be reused. |
| Apple |  | Reuse the R16 framework |
| CATT | Yes |  |
| ZTE | Yes | Reuse the current configuration within MeasIdleCarrierNR-r16. |
| Huawei, HiSilicon |  | Given the limited discussion time, we should use the Rel-16 configuration as it is, i.e. *measIdleConfig-r16* in *RRCRelease* and *measIdleConfigSIB-r16* in *SIB11*. |
| Xiaomi | Yes |  |
| LGE | Yes |  |
| MediaTek |  | Before discussing the configuration granularity, we should first understand what’s this new configuration for.For solution based on existing measurement, we are not sure whether we need this configuration. There may be a need for NW to filter which frequency to report as cell reselection measurement result may not be used for DCCA setup.For solution based on enhanced measurement (**if feasibility is concluded by RAN4**), we only need NW to indicate which EMR frequency could/should do additional measurement (i.e. reusing R16 IE with one additional bit). There is no need to have a complete list. Please also note that RAN4 is still discussing this (see R4-2317328, Issue 2-3-4) and we can wait for RAN4. |
| Qualcomm | Yes | We can reuse the Rel-16 EMR configuration as provided by *measIdleConfig-r16* in *RRCRelease* and *measIdleConfigSIB-r16* in *SIB11* with enhancements to indicate the reduced number of EMR frequencies to measure for the Rel-18 enhanced measurements, as agreed by RAN4. |
| vivo | Yes  | For enhanced measurement, R16 IE MeasIdleCarrierNR-r16 can be reused.For solution based on existing measurement, we have the similar question as MTK. It is unclear whether this solution has been considered and covered by the CR.  |
| OPPO | Yes | The current way can be reused. |
|  |  |  |
|  |  |  |

**Summary 1**: Almost all the companies agreed to use ARFCN for enhanced measurements (or also known as additional measurements). One company was pointing out correctly that RAN4 is working on both enhanced measurements as well as some additional aspects for existing measurements.

**Proposal 1**: We will continue reusing existing way of configuring ARFCN for measurements (not the band as mentioned in RAN4 LS/agreements).

The RAN4 agreements also say: *It is up to UE implementation how to select a band to report unless NW specify a band to report.*

So how this is written RAN4 seems to assume a single band is reported by the UE. Thus it seems also logical to only configure single band (ARFCN) for the UE to be measured.

**Question 2**: Would you agree that only single ARFCN is configured for additional measurements?

|  |
| --- |
| Answers to Question 2 |
| Company | Yes/No | Technical Arguments |
| CMCC |  | We are not sure whether the question is about configuration or reporting, since the RAN4 agreement is about reporting rather than configuration. Besides, it’s not clear whether ARFCN here is one-to-one mapping to the band? |
| Ericsson |  | We don’t think the configuration should be limited to only a single ARFCN. The UE should be able to report multiple frequencies in case it has measured on multiple frequencies, e.g. before initiating RRCResume. |
| Apple |  | Don’t think the Ran4 intention is reflected in the question. |
| CATT |  | We don’t think the report band means one frequency to be measured. Maybe we could ask RAN4 to clarify the relationship of the band to report and the measurement frequency. |
| ZTE |  | Not sure whether RAN4 intention is to let the NW explicitly configure a band to report, or rely on the frequencies configured to measure? It may be better to firstly ask RAN4 to clarify their intention on this agreement, e.g. whether the NW is required to configure a band to report (in addition to the configured measurement frequency), and if allowed, how many band can be configured? |
| Huawei, HiSilicon |  | We can ask RAN4 is any restriction is needed for a single ARFCN. |
| Xiaomi |  | We also think we need to check with RAN4 whether RAN4 intention is only one band to report or only one band to measure, or both. |
| LGE | No | The RAN4 agreement is about reporting, not measurements. We think RAN4 did not conclude to support extra/additional measurements(feasibility needs to be confirmed)So if we follow the RAN4 agreement, the configuration can indicate a list of frequencies in a band for which UE may report measurement results *if available*.  |
| MediaTek |  | See our comment in Q1 |
| Qualcomm | No | We do not think this restriction is needed. |
| vivo | No  | We think that the network can configure one or more ARFCNs for additional measurements, as this is also supported in Rel-16 EMR. From our understanding, if we reuse the EMR framework for additional measurement, this configuration controls both measurement and reporting.  |
| OPPO |  | We do not think the intention from RAN4 is to set a restriction on the number of bands that can be configured for additional measurement, maybe only the reporting is involved in this agreement. We can further check this understanding with RAN4. |
|  |  |  |
|  |  |  |

**Summary 2**: It seems most companies think we should not limit measurements to single frequency for additional measurements and if done so it should be questioned from RAN4. As the configuration of multiple frequencies is simple in RAN2 signaling we could start signaling design with multiple frequencies.

**Proposal 2**: Allow configuration of multiple ARFCNs for additional measurements.

The RAN4 agreements also say: *It is up to UE implementation how to select a band to report unless NW specify a band to report.*

In R16 EMR UE only reports frequencies configured by NW. Also benefits for allowing UE to report whatever ARFCN seems bit vague. Thus it would be good to understand what companies think how critical it is to cover this scenario where NW does not configure anything to be reported but UE still reports additional measurements.

**Question 3**: Would you see need to handle situation to allow UE to report additional measurements without NW configuring those?

|  |
| --- |
| Answers to Question 3 |
| Company | Yes/No | Technical Arguments |
| CMCC |  | We are wondering the exact meaning of “NW configuring those”, since based on the following RAN4’s agreements, UE may have measurement results of frequencies configured in EMR and cell reselection, and both of the two kinds of measurement are network configured and the results can be reported.

|  |
| --- |
| **RAN4 #108 Agreements:** Measurement reporting**<Agreement>*** For UE which is not capable of EMR, when the measurement results during idle/inactive mode are available and valid, UE can report these results to the network during or after RRC setup or resume procedures. The reporting procedure is up to RAN2.

**<Agreement>** * It is up to UE implementation how to select a band to report unless NW specify a band to report.
 |

 |
| Ericsson | No | We don’t think the UE should report measurements not configured by the network, as they are probably not of any use to the network in such case. Cell reselection measurements are not useful for deciding on CA/DC setup. |
| CATT | No | We think this agreement is for the additional measurement report, not including the EMR/eEMR report.We wonder whether the report band is equivalent to the measurement configuration.  |
| ZTE |  | Not sure whether “NW configuring those” means “those configured to measure” or “those configured to report”? Perhaps firstly ask RAN4 for clarification. |
| Huawei, HiSilicon | No | Same view like Ericsson. |
| Xiaomi |  | We're a little confused about “without NW configuring those”.In our understanding, we think the following cases can be considered for which frequency can be reported:* Case 1: If one ARFCN is configured to report, UE reports the measurement results of the ARFCN
* Case 2: No ARFCN is configured to report (maybe it means “without NW configuring those” in Q3 )
	+ Case 2.1: If no ARFCN is configured to measure for additional measurement, it is up to UE implementation to select a frequency to report, the frequency is one of the frequencies configured for EMR/cell reselection and whose measurement results are available
	+ Case 2.2: If one ARFCN is configured to measure for additional measurement, UE reports the measurement results of the ARFCN
	+ Case 2.3: If more than one ARFCNs are configured to measure for additional measurement, it is up to UE implementation to select a frequency indicated by one of the configured ARFCN to report.
 |
| LGE | No | Since the reporting is for CA/DC setup, it is not meaningful to report a frequency that is not supposed to be used for CA/DC from network point of view.  |
| MediaTek | No | For solution based on existing measurement, we are fine to have NW configuration to filter which frequency to report as cell reselection measurement result may not be used for DCCA setup.For solution based on enhanced measurement (**if feasibility is concluded by RAN4**), we understand there is already EMR configuration for measurement list. |
| Qualcomm | No  | Reports on frequencies not configured by the network may not be useful to the network. |
| vivo | No | Same view as Ericsson.  |
| OPPO |  | The question is not clear on “configuring those” as comments from ZTE. If it refers to measurement configuration, we think UE will not report additional measurement if UE is not configured to perform additional measurement. If it refers to the ARFCN specified by NW for reporting, we think UE can still report additional measurement since it can up to UE implementation to select a ARFCN to report as agreed by RAN4. |
|  |  |  |
|  |  |  |
|  |  |  |

**Summary 3**: It seemed that almost all the companies understood that UE should not report measurements for frequencies which are not configured but also some companies thought it might be best to check with RAN4 what they mean with “*It is up to UE implementation how to select a band to report unless NW specify a band to report.*”

**Proposal 3**: Generally in RAN2 understanding is that UE should not report something not configured by NW. Check with RAN4 what is their intention with “*It is up to UE implementation how to select a band to report unless NW specify a band to report.*”.

R16 EMR measurements are controlled by T331 timer, however these new additional measurements are not and time to perform those is defined by RAN4.

**Observation 1:** T331 does not control when UE performs FR2 idle/inactive measurements and when measurements are performed are defined in RAN4

**Question 4**: Do you agree that T331 timer (or similar) does not control R18 additional measurements?

|  |
| --- |
| Answers to Question 4 |
| Company | Yes/No | Technical Arguments |
| CMCC | Yes  | T331 starts upon receiving *RRCRelease* message with measIdleDuration, and stops upon receiving *RRCSetup, RRCResume, RRCRelease* with idle/inactive measurement configuration, while additional measurements may be performed during RRC setup/resume procedure (upon receiving *RRCsetup, RRCResume*). Besides, T331 may expire if the time between UE RRC\_IDLE and UE RRC\_CONNECTED is too long. Therefore, T331 is not suitable to control R18 additional measurements. What’s more, RAN4 has defined the starting point and end point of the enhanced measurement, thus, there’s no need to introduce an extra timer for this. |
| Ericsson |  | According to 5.7.8.3 the UE releases the dedicated measurement configuration when T331 expires. The UE may continue measuring according to what is defined in SIB. If the rel-18 measurement configuration is included in the SIB, the UE may perform the rel-18 measurements even after T331 has expired, assuming the legacy behaviour is reused for rel-18.  |
| Apple | Yes, but | We believe in the same theme as allowing the UE to decide on what to do. |
| CATT | Yes | We think the EMR and the additional measurement is independent. So the T331 doesn’t control the additional measurements.If EMR procedure is one condition of triggering additional measurement, the T331 may have impact on additional measurements. But we can revise the agreement if RAN4 have such progress. |
| ZTE |  | If the R18 additional measurement is independent from R16 EMR, we agree that T331 doesn’t control the additional measurement.If the R18 additional measurements is performed based on R16 EMR, we share the same view with Ericsson, i.e reuse the EMR similar mechanism after T331 expiry. |
| Huawei, HiSilicon |  | For simplicity, it is desirable to reuse the existing procedure and it seems to be ok: before T331 expiry, the UE will use the dedicated configuration, after T331 expiry, it will use the configuration in SIB11 only, but up to UE implementation to do the measurements or not. |
| Xiaomi | Yes | For Rel-18 additional measurements, R4 has reached some agreements for the start point and the stop point, hence T331 based control is not needed. |
| LGE | Yes |  |
| MediaTek | No | For solution based on existing measurement, there is no T331.For solution based on enhanced measurement (**if feasibility is concluded by RAN4**), we don’t think RAN4 agreed to remove T331. It is not preferred to mandate UE to do more measurement in IDLE/INACTIVE mode. The current procedure (as mentioned by HW) is workable. |
| Qualcomm | Yes | Agree with CATT and Xiaomi that since RAN4 has defined the start and end points for the Rel-18 enhanced measurements, a timer is not needed to control the time for which the Rel-18 enhanced measurements are done. |
| vivo | Yes | Agree with Ericsson, Huawei that we can reuse the existing EMR procedure as much as possible. Maybe a note is sufficient.  |
| OPPO |  | It depends on whether the EMR and R18 additional measurement are independent features. |
|  |  |  |
|  |  |  |

**Summary 4**: It seemed to be general understanding additional measurements are not controlled by T331 (but any measurements based on R16 EMR are even if enhanced in R18).

**Proposal 4**: Enhanced measurements are not controlled by T331 but when UE does measurements are defined by RAN4 explicitly.

RAN4 does not state any limitations either that R16 idle/inactive measurements could not be configured simultaneously with new R18 FR2 idle/inactive measurements. Thus we need to allow this kind of configuration and procedural text.

**Question 5**: Do you agree that Configuration of R18 FR2 idle/inactive measurements are allowed to be configured simultaneously with R16 idle/inactive measurements?

|  |
| --- |
| Answers to Question 5 |
| Company | Yes/No | Technical Arguments |
| CMCC | Yes |  |
| Ericsson | Yes | We assume this means that rel-18 configuration is done per carrier. |
| Apple | Yes |  |
| CATT | Yes |  |
| ZTE | Yes |  |
| Huawei, HiSilicon |  | We should make it simple, e.g.- there is a single dedicated (in RRCRelease) and broadcast (in SBI11) configuration that applies for Rel-16 and Rel-18 measurements, and it can be the legacy configuration- If the UE is configured to perform Rel-18 measurements and the camping cell wants Rel-18 measurements (SIB1), the UE only performs Rel-18 measurements- If the UE is configured to perform Rel-18 measurements and the camping cell only wants Rel-16 measurements (SIB1), the UE performs Rel-16 measurements |
| Xiaomi | Yes |  |
| LGE | Yes |  |
| MediaTek |  | We tend to agree with Huawei.For solution based on enhanced measurement (**if feasibility is concluded by RAN4**), there could be one control bit (per UE or per frequency) to indicate whether to perform the additional measurement. |
| Qualcomm | Yes |  |
| vivo | Yes  |  |
| OPPO | Yes |  |
|  |  |  |
|  |  |  |

**Summary 5**: Almost all the companies seemed to agree that additional measurements can be configured simultaneously with R16 EMR measurements. 2 companies considered that we could just indicate in the R16 EMR with additional bits for which frequencies additional measurents are applicable. RAPPORTEUR additional input: It should be noted like Mediatek informed also earlier tha RAN4 are working on “additional measurements” as well as “enhancements for existing measurements”. Thus it seems quite difficult to mix the configuration of existing and additional measurements.

**Proposal 5**: Allow configuring additional measurements and EMR measurements separately.

Then the LSes from RAN4 does not take stance whether we need to configure the frequency to be measured in dedicated signaling or broadcast signaling. At least we have following choices:

1. Only enable measurements in dedicated signaling and measured frequency comes in broadcast signaling
2. Enable and configure measured frequency in dedicated signaling
3. Enable and configure measured frequency in broadcast signaling
4. Configure measured frequency in dedicated signaling and enable measurements in broadcast signaling

In R16 idle/inactive measurements one configures UE to do idle/inactive measurements in *RRCRelease* and also NW can configure which frequencies to measure. Frequencies to be measured are updated with broadcast signaling i.e. if SIB11 is present it overrides measured frequencies. It would seem quite natural to go this way or then purely limit configuration to *RRCRelease* which would simplify the procedural text.

**Question 6**: Do you agree to configure FR2 idle/inactive measurements in RRCRelease and also SIB configuration to update measured frequency (similar to R16 EMR)?

|  |
| --- |
| Answers to Question 6 |
| Company | Yes/No | Technical Arguments |
| CMCC | Yes | Similar approach to R16 EMR can be used, but we prefer that network can provide more information to UE, such as a threshold for UE to decide whether the measurement for a specific frequency is needed (also discussed in Q11). |
| Ericsson |  | We don’t agree with the rapporteur view that SIB11 overrides the dedicated signalling. We think that what was signalled in dedicated signalling is applicable as long as T331 is running. After T331 has expired or if the UE didn’t receive anything in dedicated signalling, the UE will look at SIB11. We agree to configure rel-18 measurements in RRCRelease and SIB11 as for rel-16, and we also support CMCC proposal to add more information to the UE, such as threshold. |
| CATT |  | We agree with Ericsson, the SIB11 configuration doesn’t override the measurement configuration configured via dedicated signalling.But we agree the R16 mechanism could be reused for R18. |
| ZTE |  | Regarding how to update the measurement configuration via those in SIB configuration, we share the same view with Ericsson, i.e. reuse the same mechanism as R16 EMR.Besides, we also support CMCC’s proposal to provide more information to the UE, e.g. threshold to control the measurement for a specific frequency.  |
| Huawei, HiSilicon |  | The existing Rel-16 procedures should apply to Rel-18 measurements, including those related to configuration.We can consider additional parameters but we should keep complexity low. |
| Xiaomi |  | Agree to reuse Rel-16 EMR mechanism. |
| LGE | See comments | We prefer to make this feature as simple as possible, and RAN2 only needs to support signalling for which RAN4 progress is mature enough. Given that the configuration is only about a list of frequencies for which reporting is welcome, broadcast configuration seems sufficient. The necessity of dedicated configuration is unclear.  |
| MediaTek | No | Similar comment as Q5, we prefer to reuse original R16 IE and procedure.For solution based on enhanced measurement (**if feasibility is concluded by RAN4**), there could be one control bit (per UE or per frequency) to indicate whether to perform the additional measurement. |
| Qualcomm | Please see comments | We agree with Ericsson’s understanding that SIB11 doesn’t override the dedicated signalling.For the Rel-18 enhanced measurements, the Rel-16 RRCRelease or the Rel-16 SIB11 based configuration can be used. However, if the configuration is to be provided using both Rel-16 RRCRelease and SIB11, then a mechanism needs to be defined as to when UE uses each configuration.  |
| vivo | Yes | FR2 idle/inactive measurement can be configured via RRCRelease and SIB, and SIB11 configuration doesn’t overrides the dedicated signalling measurement configuration, which is similar to R16 EMR. Besides, we agree with CMCC that network can provide more information to UE, such as a threshold. |
| OPPO |  | We agree that the R16 EMR mechanism can be reused for the configuration of additional measurement, i.e., the measurement configuration for additional measurement can be configured via RRCRelease or SIB.  |
|  |  |  |
|  |  |  |
|  |  |  |

**Summary 6**: Almost all the companies considered that we can reuse basic principle of configuring to be measured frequencies for additional measurements in RRCRelease and also SIB – procedure when UE applies SIB frequencies could follow similar principles as for R16 EMR.

**Proposal 6**: R16 EMR principles of configuring measured frequencies via *RRCRelease* and SIB is used for additional measurements. Also similar “procedure” is used when measured frequencies are updated from SIBs as used for R16 EMR..

## 4.2 Reporting of measurement availability

Normally we don’t allow UE to send signaling to NW that it does not support. In R16 idle/inactive measurements UE reporting of availability of measurements is controlled with presence of SIB11 which include which frequencies to measure. It seems logical to follow similar route for FR2 measurements. If allowed in SIB1 to report the measurements, then UE will report availability R16 idle/inactive measurements in the *RRCResumeComplete* or *RRCSetupComplete.* It would seem also logical to do this for FR2 type of measurements.

**Question 7**: Do you agree UE may only report available FR2 measurements to nw if indicated to continue measurements in SIB1 and reporting can be done in either in the *RRCResumeComplete* or *RRCSetupComplete* (i.e. similarly to *idleModeMeasurementsNR*)?

|  |
| --- |
| Answers to Question 7 |
| Company | Yes/No | Technical Arguments |
| CMCC | Yes | Similar approach to Rel-16 can be reused. |
| Ericsson | Yes | Reporting of measurement availability in RRCResumeComplete and RRCSetupComplete. |
| Apple |  | Only reporting of measurement availability  |
| CATT | Yes |  |
| ZTE | Yes | Reporting of measurement availability in RRCResumeComplete and RRCSetupComplete. |
| Huawei, HiSilicon |  | This should follow Rel-16 procedures exactly |
| Xiaomi | Yes |  |
| LGE | Yes | Similar approach to Rel-16 can be reused. If only broadcast configuration is used, network can blindly request reporting measurement results via RRCResume based only on the relevant UE capability, i.e. there is no problem to reuse R16 indication/reporting approaches. |
| MediaTek |  | For solution based on existing measurement, Rel-16 procedure should be reused to report the availability.For solution based on enhanced measurement (**if feasibility is concluded by RAN4**), the availability may be reported in *RRCResumeComplete* or *RRCSetupComplete* if the UE has completed the additional measurement.And we think the R18 solution should be common for FR1 and FR2, it is not clear to us why we want to limit it to FR2 only. |
| Qualcomm | Yes | The Rel-16 procedure can be followed for this. |
| vivo | Yes | Reporting the availability of R16 idle/inactive measurements can be reused. The specific procedure and wording can align R16. |
| OPPO | Yes |  |
|  |  |  |
|  |  |  |

**Summary 7**: It seemed companies agreed to only report available additional measurements to NW if indicated to continue measurements in SIB1 and reporting can be done in either in the RRCResumeComplete or RRCSetupComplete (i.e. similarly to idleModeMeasurementsNR)

**Proposal 7**: UE only reports available additional measurements to NW if indicated to continue measurements in SIB1 and reporting can be done in either in the RRCResumeComplete or RRCSetupComplete (i.e. similarly to idleModeMeasurementsNR).

In Rel-16, UE indicates that it has **some** measurement results available at connection setup. RAN4 has agreed to discuss in parallel two solutions to improve SCell setup time: *1)* *without additional measurements* and *2)* *with additional measurements*.

Based on RAN4 agremeents UE may (and likely will) continue measurements even after RRCResume/SetupComplete when UE does not yet have measurements at time of sending RRC resume/setup complete – in below we list different cases that may occur:

1. UE does not have any measurements available at RRC setup/resume complete
	* UE does not continue enhanced measurements for FR2
	* UE continues enhanced measurements for FR2
2. UE has measurements available at time of RRC setup/resume complete
	* UE does not continue enhanced measurements for FR2
	* UE continues enhanced measurements for FR2

Thus it seems following cases may occur when sending RRC setup/resume Complete messages:

1. Measurements available (UE is ready to report)
2. Measurements ongoing (UE needs more time before it will be ready to report)

Case 1 applies when the UE is not performing additional measurements (because may not have such capability or because the available measurements are considered sufficient without the need for additional measurements). Case 2 Applies to a UE that has measurements available from IDLE/INACTIVE mode, and the UE will continue enhanced measurements for some time during connected mode.

One of the reasons to have the different options is that once the T331 timer has been expired, it is up to UE implementation to perform measurements. In some scenarios when the MSG-1 or Paging message arrives to UE, the UE may need some (e.g., one or two) extra samples to meet the measurement reporting requirements. Depending on the duration of the RRC procedure, these measurement may be finished or not, and therefore, the network needs to know if there are carrier(s) that are being measured.

Therefore, the difference to R16 idle/inactive measurements is that UE may not yet have measurement results available at this point, especially if UE doing enhanced measurements which may continue beyond the point of sending the response message to the network for connection resume/setup. This could also occur in case the FR2 SMTC window is long (e.g. 80 or 160 ms) and UE is still waiting for the measurement occasion during SMTC when the RRC connection setup/resume procedure ends.

**Proposal 5:** UE reports availability and/or ongoing of FR2 measurements (which may also include information about measured carriers) in *RRCResumeComplete* or *RRCSetupComplete*

**Question 8**: Do you agree that UE needs to availability (similar to R16 EMR) and/or ongoing of FR2 measurements (Not in R16 EMR) in *RRCResumeComplete* or *RRCSetupComplete*?

|  |
| --- |
| Answers to Question 8 |
| Company | Yes/No | Technical Arguments |
| CMCC | Partly Yes | Based on RAN4’s agreements, the ending point of enhanced measurement at the reception of the RRC CONNECTED mode measurement configuration (the 1st RRC\_reconfiguration message) is clearly defined. Though the measurement may be ongoing at the time of *RRCResumeComplete* or *RRCSetupComplete,* it will end at the time of the 1st RRC\_reconfiguration message, therefore, we think only reporting availability is sufficient. |
| Ericsson | No | We agree with CMCC that the ending point of the rel-18 measurements should be when the connected mode measurement configuration is received. However, in the RRC resume procedure, the connected mode measurement configuration can be included already in the RRCResume message and the EMR results may be included in the RRCResumeComplete message. So we think the UE can indicate the availability of the measurements as in rel-16, but we don’t see any reason to indicate that measurements are ongoing as the connected mode measurements may already be ongoing. |
| CATT | No | The availability indication is enough. Agree with Ericsson.  |
| ZTE | No | Agree with CMCC and Ericsson that reporting availability is enough, no need to introduce ongoing indicator. |
| Huawei, HiSilicon |  | We are not sure what the question means exactly. Does it mean"if the UE has Rel-16 measurement results or if the UE is still doing measurements (for RRCSetupComplete only), the UE set the Rel-16 indication?"In our understanding, a separate one-bit indication for "the UE is still doing Rel-18 measurements" could be useful in the RRCSetupComplete so that the network does not request results before providing the RRC\_CONNECTED measurement configuration, but no strong view. |
| Xiaomi | No | Agree to report “availability”. “Ongoing” flag is not needed. |
| LGE | See comments | We think a) “ongoing” may be continuation of measurements done for cell reselection and b) “ongoing” may be continuation of extra measurements that has started upon initiation of RRC setup/resume (MT/MO). For both cases a) and b), the value of ‘ongoing’ measurement (i.e., extra measurement) does not seem high, given that the extra measurement duration is short (it terminates upon first reconfiguration). * If it is the case a), the chance is not high that inaccurate measurement results done for cell reselection becomes accurate by performing extra measurements.
* If it is the case b), the chance to obtain accurate measurements via extra measurements is lower than case a) because the initiation of measurements was only upon connection setup/resume. Furthermore, we think RAN4 did not make final conclusion whether to support it or not ; RAN4 still requires confirmation on feasibility and benefit of the extra measurement.

But, from pure signalling point of view, the ‘ongoing’ indication, if introduced needs to be included in RRCSetupComplete or RRCResumeComplete |
| MediaTek | No | For solution based on existing measurement, “on-going” indicator is clear not needed.For solution based on enhanced measurement (**if feasibility is concluded by RAN4**), we agree with Ericsson this “on-going” indicator seems not useful. |
| Qualcomm | No | The Rel-16 indication is fine, but there is no need for the additional “ongoing” indication, as many other companies have pointed out above. |
| vivo | No | Agree with CMCC and Ericsson that the availability indication is enough. |
| OPPO | No | The availability indication is enough. |
|  |  |  |
|  |  |  |
|  |  |  |

**Summary 8**: Almost every company agreed that we only report availability of the measurements. Although it was not clear that how NW will know to request additional measurements if they are not available yet when availability is indicated in in *RRCResumeComplete* or *RRCSetupComplete*

**Proposal 8**: UE may indicated availability of additional measurements in the in *RRCResumeComplete* or *RRCSetupComplete.* FFS whether there is need to indicate additional measurements are continued after sending in *RRCResumeComplete* or *RRCSetupComplete (see question/proposal 10 for possible answer)*

## 4.2 Request and Report of Measurements

Rel-16 reporting is based on UE indicating it has some measurement available, then the network requests the measurements and UE responses. When the UE is allowed to continue the measurements in the CONNECTED mode, the network does not know the exact time when the UE has finished the measurements, apart from the time duration that is specified as RAN4 minimum requirements for the measurements. For the reporting, one option would be to allow UE to trigger measurement report once it has finished the FR2 measurements. Alternatively, the network may wait until the time defined in the minimum requirements has passed and request the measurement results indicated by UE.

For R16 idle/inactive measurements NW can request measurement reporting in two ways:

* + 1. In resume procedure as part of *RRCResume* i.e. *idleModeMeasurementReq*
		2. *UEInformationRequest* with *idleModeMeasurementReq*

Resume message request was also done in R16 to speed up measurement reporting for resume case where NW already knows early about UE capability. It would seem we could follow similar principle for R18 FR2 reporting request. Then it becomes natural to report measurements with either *RRCResumeComplete* or *UEInformationResponse*

**Question 9**: Do you agree to use *UEInformationRequest* procedure to request UE to report available measurements and UE reports measurements in *UEInformationResponse* and additionally allow *RRCResume* to request UE to report measurements and UE reports measurements in *RRCResumeComplete*? (similarly to R16 EMR)

|  |
| --- |
| Answers to Question 9 |
| Company | Yes/No | Technical Arguments |
| CMCC | Yes |  |
| Ericsson | Yes |  |
| CATT | Yes |  |
| ZTE | Yes |  |
| Huawei, HiSilicon |  | If the existing procedure is used unmodified, yes. |
| Xiaomi | Yes |  |
| LGE | Yes |  |
| MediaTek |  | We think this part we could completely reuse R16 procedure and IE. |
| Qualcomm | Yes |  |
| vivo | Yes  |  |
| OPPO | Yes |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Summary 9**: Everobody agreed to reuse R16 procedure.

**Proposal 9**: We will use *UEInformationRequest* procedure to request UE to report available additional measurements and UE reports measurements in *UEInformationResponse* and additionally allow *RRCResume* to request UE to report measurements and UE reports measurements in *RRCResumeComplete* (similar to R16 EMR)

As discussed earlier UE may continue enhanced FR2 measurements until *RRCReconfiguration* as seen from RAN4 agreements:*The ending point of enhanced measurement at the reception of the RRC CONNECTED mode measurement configuration (the 1st RRC\_reconfiguration message)*

For RAN2 this does not really pose any limitation as such but likely just information for NW that I may not make sense to request results much after 1st reconfiguration. But it seems feasible that NW may request UE to report measurement results to NW soon after it gets indication that UE is continuing to do measurements after sending resume/setup complete message. If UE does not at time of request (*UeInformationRequest)* yet have measurement results it could just report those when ready even after reception of *RRCReconfiguration.* So there is no need to in RAN2 to consider when UE is doing measurements.

**Proposal 8:**

**Question 10**: Do you see that UE should report the measurements as soon as they are available if requested by NW with *UEInformationRequest?*

|  |
| --- |
| Answers to Question 10 |
| Company | Yes/No | Technical Arguments |
| CMCC | Yes | In our understanding, if only availability (rather than ongoing) reporting is supported, once availability is reported by UE, it means UE has the measurement results, and it can report the measurement results as soon as possible if request by the network. |
| Ericsson | Yes | The connected mode measurement configuration can also be received in RRCResume, i.e. not only RRCReconfiguration. We agree with CMCC that if the UE has indicated availability, the UE will report them when the network requests them. |
| CATT | Yes |  |
| ZTE | Yes |  |
| Huawei, HiSilicon |  | Does "report the measurements as soon as they are available if requested by NW with *UEInformationRequest*" mean:1) upon receiving UEInformationRequest, the UE immediately replies with available measurement results; or2) upon receiving UEInformationRequest, if the UE has not finished performing the measurements, the UE finishes the measurements and then replies with available measurement resultsWe think 1) is the legacy behaviour and it should be reused. |
| Xiaomi | Yes  | Yes, if only “availability” indication in Q8 is supported  |
| LGE | No | For indication of “available”, the answer is obviously Yes. The question is non-trivial for indication of “ongoing”, and for this case, the question asks whether to introduce delayed triggering of “UEInformationResponse”. We prefer to allow UE to indicate “available” via UAI such that network can trigger UE information procedure upon receiving the UAI. This is more clean and consistent with existing UE behaviours regarding UE information procedure  |
| MediaTek |  | Don’t quite understand the question. But we tend to think behavior 1) mentioned by Huawei is the intended one.  |
| Qualcomm | Yes | Agree with Huawei about UE immediately reporting with available measurement results upon receiving UEInformationRequest. |
| vivo |  | Not sure we understand this question. In our understanding, after UE received the request form the network, if UE has available measurement result, UE reports measurements in *UEInformationResponse*. |
| OPPO | Yes |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Summary 10**: It seemed to be general understanding that when UE gets UEInformationRequest to report possible available measurement results UE immediately sends the report. But it seemed that if UE is still doing measurements and they are not available it is not clear which kind of procedure is used.

**Proposal 10**: Whenever NW requests additional measurement results with *UEInformationRequest* UE reports results with *UEInformationResponse* (same as R16 EMR). FFS how measurements are sent to NW if UE is still doing measurements and they are not yet available when requested by NW.

And here to collect if you have any other questions in mind that need clarifying:

**Question 11**: Please list here any other aspects you want to be discussed

|  |
| --- |
| Answers to Question 11 |
| Company | Yes/No | Technical Arguments |
| CMCC | Yes | **Introduction of thresholds reduce the number of carriers to be measures for fast Scell/SCG setup（Proposed in** **R2-231048）**In RAN4 LS R2-2309462/R4-2314466, one agreement is about reducing the number of measurement carriers:

|  |
| --- |
| **RAN4 #104-e R4-2214348** **<Agreement>:*** Reduce the number of EMR carriers to be measured for improved measurement.
 |

In our understanding, the time during RRC setup/resume procedure is around tens of ms, which may be not enough to complete the measurement of all the EMR carriers. Since the measurement delay is scaled with the number of carrier, we think some thresholds can be introduced to reduce the number of carriers to be measured, which makes the measurement delay reduced and the results reported by UE more valid, and further enables a fast SCell/SCG setup. |
| Ericsson | Yes | We agree with the proposal from CMCC to add threshold.According to the rel-18 WID, the validity of existing measurements should be addressed also. RAN4 made an agreement that the network can configure a validity time, that the UE should only send measurements if they are less old than the configured value. This needs to be added in RAN2 specifications. In addition, for the network to know the validity of the reported measurements, we the UE should include information about the time difference between when the measurements were performed and when they were reported. |
| ZTE | Yes | We agree with CMCC’s proposal to introduce the threshold. |
| Huawei, HiSilicon |  | Ok to consider a new parameter but we should keep complexity low. |
| Xiaomi |  | Ok to discuss how to reduce the number of EMR carriers to be measured for improved measurement |
| MediaTek |  | On CMCC proposal, we have the same comment as Huawei |
| Qualcomm |  | The network should explicitly configure the set of frequencies (carriers) for which it wants the UE to perform the Rel-18 enhanced measurements and provide measurement reports. Therefore, we do not support the threshold-based mechanism suggested by CMCC and think that it is an unnecessary optimization. RAN4 has agreed that it is up to UE implementation to determine what to report if network does not configure anything.  |
| vivo |  | Agree with the proposal from CMCC.  |
| CMCC |  | Agree with Ericsson’s proposal to consider including the information about the time difference between when the measurements were performed and when they were reported. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Summary 11**: There were proposal to enhance additional measurements by e.g. configuring threshold to control what frequencies are used for measurements as well as reporting time difference between when measurements were performed and reported..

**Proposal 11**: FFS whether we need to have threshold to control which carriers are to be measured by UE and whether we need to report time difference between when the measurements were performed and when they were reported.

# 5 TP

In the Annex a TP is provided taking R16 EMR as baseline. In th TP similar ASN.1 naming was used but it might be better in the end to differentiate ASN.1 field names from R16 EMR. So this question here is to collect any general comments on how to implement CR. It should be noted that the TP takes some questions above as agreeable in order to be able to write the CR – naturally TP needs to be updated once the RAN2 understanding on the details is established:

**Question 12**: Any comments on the TP are welcome here:

|  |
| --- |
| Answers to Question 12 |
| Company | Yes/No | Technical Arguments |
| Ericsson | Yes | The conclusion from RAN2#123bis was to reuse the EMR procedures and signalling to a great extent. This is not the case in the TP below, where new rel-18 parts are added in most places. We think rel-16 EMR specification can be reused a lot more, e.g. by adding an extension for rel-18 where needed. |
| Huawei, HiSilicon |  | EMR procedures and signalling should be reused with less modifications.It could be sufficient to:1) add a UE capability to say the UE supports Rel-18 measurements2) add one bit in MeasIdleConfigDedicated to indicate that the UE shall do Rel-18 measurements3) add one bit in SIB1 to indicate that the UE shall perform and report Rel-18 measurements if configured to do so4) add one bit in RRCConnectionSetupComplete (to indicate the UE is doing Rel-18 measurements so the network will not fetch results before providing the measConfig for RRC\_CONNECTED)5) Specify that if the UE is configured to perform Rel-18 measurements and SIB1 indicates that the network wants Rel-18 measurements, the UE performs Rel-18 measurements and not 5.7.8.2a. Otherwise, the UE follows 5.7.8.2a. |
| MediaTek |  | We think current CR is too complicate. Since RAN2 has agreed to reuse EMR as much as possible, we should not duplicate EMR configuration to Rel-18. Huawei approach 1) to 4) could be considered as a starting point if the feasibility of solution based on enhanced measurement is concluded by RAN4. |
| vivo |  | Basically, agree with MTK. Moreover, RAN4 discussed two solutions in parallel:1. Solution based on existing measurement.2. Solution based on enhanced measurement.The current CR seems not cover the Solution based on existing measurement.  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Summary 12**: It seems that few companies would prefer to add extension of for R18 eEMR measurements instead of having new R18 IE. As indicated also consider then how one would then allow separately configuring both R18 and R16 EMR measurements as well as R18 measurements may be based on existing measurements or enhanced measurements.

**Proposal 12**: Rapporteur hopes companies bring alternative ways to capture R18 EMR measurements i.e. measurements using existing measurements as well as measurements using enchaned (additional) measurements and how they are kept separate from R16 EMR measurements..

# 6 RAN4

In RAN2#123bis there were comments that some aspects may need clarification or more progress in RAN4 thus in order to see if we need to have LS to RAN4:

**Question 13**: If you see some aspects need to be asked/clarified from RAN4 please list those

|  |
| --- |
| Answers to Question 13 |
| Company | Yes/No | Technical Arguments |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Summary 13**: No separate comments on this section.

**Proposal 13**: No separate comments on this section but based on other proposals there seems to be few issues that may need clarification from RAN4.

# 7 Conclusion

**Proposal 1**: We will continue reusing existing way of configuring ARFCN for measurements (not the band as mentioned in RAN4 LS/agreements).

**Proposal 2**: Allow configuration of multiple ARFCNs for additional measurements.

**Proposal 3**: Generally in RAN2 understanding is that UE should not report something not configured by NW. Check with RAN4 what is their intention with “*It is up to UE implementation how to select a band to report unless NW specify a band to report.*”.

**Proposal 4**: Enhanced measurements are not controlled by T331 but when UE does measurements are defined by RAN4.

**Proposal 5**: Allow configuring additional measurements and EMR measurements separately.

**Proposal 6**: R16 EMR principles of configuring measured frequencies via *RRCRelease* and SIB is used for additional measurements. Also similar “procedure” is used when measured frequencies are updated from SIBs as used for R16 EMR..

**Proposal 7**: UE only reports available additional measurements to NW if indicated to continue measurements in SIB1 and reporting can be done in either in the *RRCResumeComplete* or *RRCSetupComplete* (i.e. similarly to idleModeMeasurementsNR).

**Proposal 8**: UE may indicate availability of additional measurements in the in *RRCResumeComplete* or *RRCSetupComplete.* FFS whether there is need to indicate additional measurements are continued after sending in *RRCResumeComplete* or *RRCSetupComplete (see question/proposal 10 for possible answer)*

**Proposal 9**: We will use *UEInformationRequest* procedure to request UE to report available additional measurements and UE reports measurements in *UEInformationResponse* and additionally allow *RRCResume* to request UE to report measurements and UE reports measurements in *RRCResumeComplete* (similar to R16 EMR)

**Proposal 10**: Whenever NW requests additional measurement results with *UEInformationRequest* UE reports results with *UEInformationResponse* (same as R16 EMR). FFS how measurements are sent to NW if UE is still doing measurements and they are not yet available when requested by NW.

**Proposal 11**: FFS whether we need to have threshold to control which carriers are to be measured by UE and whether we need to report time difference between when the measurements were performed and when they were reported.

**Proposal 12**: Rapporteur hopes companies bring alternative ways to capture R18 EMR measurements i.e. measurements using existing measurements as well as measurements using enchaned (additional) measurements and how they are kept separate from R16 EMR measurements..

**Proposal 13**: No separate comments on this section but based on other proposals there seems to be few issues that may need clarification from RAN4.

.

Annex: TP for implementing eEMR

*First Modified Subclause*

5.2.2.4.12 Actions upon reception of *SIB11*

Upon receiving *SIB11*, the UE shall:

1. if in RRC\_IDLE or RRC\_INACTIVE, and UE is configured with *varMeasIdleConfig-r18;* or

1> if in RRC\_IDLE or RRC\_INACTIVE, and T331 is running:

2> perform the actions as specified in 5.7.8.1a;

*Next Modified Subclause*

5.3.3 RRC connection establishment

5.3.3.1 General

****

**Figure 5.3.3.1-1: RRC connection establishment, successful**

****

**Figure 5.3.3.1-2: RRC connection establishment, network reject**

The purpose of this procedure is to establish an RRC connection. RRC connection establishment involves SRB1 establishment. The procedure is also used to transfer the initial NAS dedicated information/ message from the UE to the network.

The network applies the procedure e.g.as follows:

- When establishing an RRC connection;

- When UE is resuming or re-establishing an RRC connection, and the network is not able to retrieve or verify the UE context. In this case, UE receives *RRCSetup* and responds with *RRCSetupComplete*.

5.3.3.1a Conditions for establishing RRC Connection for NR sidelink communication/discovery/V2X sidelink communication

For NR sidelink communication/discovery, an RRC connection establishment is initiated only in the following cases:

1> if configured by upper layers to transmit NR sidelink communication/discovery and related data is available for transmission:

2> if the frequency on which the UE is configured to transmit NR sidelink communication is included in *sl-FreqInfoList* within *SIB12* provided by the cell on which the UE camps; and if the valid version of *SIB12* does not include *sl-TxPoolSelectedNormal* for the concerned frequency; or

2> if the frequency on which the UE is configured to transmit NR sidelink discovery is included in *sl-FreqInfoList* within *SIB12* provided by the cell on which the UE camps; and if the valid version of *SIB12* includes neither *sl-DiscTxPoolSelected* nor *sl-TxPoolSelectedNormal* for the concerned frequency;

For L2 U2N Relay UE in RRC\_IDLE, an RRC connection establishment is initiated in the following cases:

1> if any message is received from a L2 U2N Remote UE via SL-RLC0 as specified in 9.1.1.4 or SL-RLC1 as specified in 9.2.4;

For V2X sidelink communication, an RRC connection is initiated only when the conditions specified for V2X sidelink communication in clause 5.3.3.1a of TS 36.331 [10] are met.

NOTE: Upper layers initiate an RRC connection (except if the RRC connection is initiated at the L2 U2N Relay UE upon reception of a message from a L2 U2N Remote UE via SL-RLC0 or SL-RLC1). The interaction with NAS is left to UE implementation.

5.3.3.2 Initiation

The UE initiates the procedure when upper layers request establishment of an RRC connection while the UE is in RRC\_IDLE and it has acquired essential system information, or for sidelink communication as specified in clause 5.3.3.1a.

The UE shall ensure having valid and up to date essential system information as specified in clause 5.2.2.2 before initiating this procedure.

Upon initiation of the procedure, the UE shall:

1> if the upper layers provide an Access Category and one or more Access Identities upon requesting establishment of an RRC connection:

2> perform the unified access control procedure as specified in 5.3.14 using the Access Category and Access Identities provided by upper layers;

3> if the access attempt is barred, the procedure ends;

1> if the upper layers provide NSAG information and one or more S-NSSAI(s) triggering the access attempt (TS 23.501 [32] and TS 24.501 [23]):

2> apply the NSAG with highest NSAG priority among the NSAGs that are included in *SIB1* (i.e., in *FeatureCombination* and in *RA-PrioritizationSliceInfo*)*,* and that are associated with the S-NSSAI(s) triggering the access attempt, in the Random Access procedure (TS 38.321 [3], clause 5.1);

1> if the UE is acting as L2 U2N Remote UE:

2> establish a SRAP entity as specified in TS 38.351 [66], if no SRAP entity has been established;

2> apply the specified configuration of SL-RLC0 as specified in 9.1.1.4;

2> apply the SDAP configuration and PDCP configuration as specified in 9.1.1.2 for SRB0;

1> else:

2> apply the default L1 parameter values as specified in corresponding physical layer specifications except for the parameters for which values are provided in *SIB1*;

2> apply the default MAC Cell Group configuration as specified in 9.2.2;

2> apply the CCCH configuration as specified in 9.1.1.2;

2> apply the *timeAlignmentTimerCommon* included in *SIB1*;

1> start timer T300;

*Next Modified Subclause*

5.3.3.4 Reception of the *RRCSetup* by the UE

The UE shall perform the following actions upon reception of the *RRCSetup*:

1> if the *RRCSetup* is received in response to an *RRCReestablishmentRequest*; or

1> if the *RRCSetup* is received in response to an *RRCResumeRequest* or *RRCResumeRequest1*:

2> if *sdt-MAC-PHY-CG-Config* is configured:

3> instruct the MAC entity to stop the *cg-SDT-TimeAlignmentTimer*, if it is running;

3> instruct the MAC entity to start the *timeAlignmentTimer* associated with the PTAG*,* if it is not running;

2> if *srs-PosRRC-InactiveConfig* is configured:

3> instruct the MAC entity to stop the *inactivePosSRS-TimeAlignmentTimer*, if it is running;

2> discard any stored UE Inactive AS context and *suspendConfig*;

2> discard any current AS security context including the KRRCenc key, the KRRCint key, the KUPint key and the KUPenc key;

2> release radio resources for all established RBs except SRB0 and broadcast MRBs, including release of the RLC entities, of the associated PDCP entities and of SDAP;

2> release the RRC configuration except for the default L1 parameter values, default MAC Cell Group configuration, CCCH configuration and broadcast MRBs;

2> indicate to upper layers fallback of the RRC connection;

2> discard any application layer measurement reports which were not transmitted yet;

2> inform upper layers about the release of all application layer measurement configurations;

2> stop timer T380, if running;

1> perform the cell group configuration procedure in accordance with the received *masterCellGroup* and as specified in 5.3.5.5;

1> perform the radio bearer configuration procedure in accordance with the received *radioBearerConfig* and as specified in 5.3.5.6;

1> if stored, discard the cell reselection priority information provided by the *cellReselectionPriorities* or inherited from another RAT;

1> stop timer T300, T301, T319;

1> if T319a is running:

2> stop T319a;

2> consider SDT procedure is not ongoing;

1> if T390 is running:

2> stop timer T390 for all access categories;

2> perform the actions as specified in 5.3.14.4;

1> if T302 is running:

2> stop timer T302;

2> perform the actions as specified in 5.3.14.4;

1> stop timer T320, if running;

1> if the *RRCSetup* is received in response to an *RRCResumeRequest*, *RRCResumeRequest1* or *RRCSetupRequest*:

2> if T331 is running:

3> stop timer T331;

3> perform the actions as specified in 5.7.8.3;

2> enter RRC\_CONNECTED;

2> stop the cell re-selection procedure;

2> stop relay (re)selection procedure if any for L2 U2N Remote UE;

1> consider the current cell to be the PCell;

1> perform the L2 U2N Remote UE configuration procedure in accordance with the received *sl-L2RemoteUE-Config* as specified in 5.3.5.16;

1> perform the sidelink dedicated configuration procedure in accordance with the received *sl-ConfigDedicatedNR* as specified in 5.3.5.14;

1> if the UE has radio link failure or handover failure information available in *VarRLF-Report* and if the RPLMN is included in *plmn-IdentityList* stored in *VarRLF-Report*:

2> if *reconnectCellId* in *VarRLF-Report* is not set after failing to perform reestablishment:

3> if the UE supports RLF-Report for conditional handover and if *choCellId* in *VarRLF-Report* is set:

4> set *timeUntilReconnection* in *VarRLF-Report* to the time that elapsed since the radio link failure or handover failure experienced in the *failedPCellId* stored in *VarRLF-Report*;

3> else:

4> set *timeUntilReconnection* in *VarRLF-Report* to the time that elapsed since the last radio link failure or handover failure;

3> set *nrReconnectCellId* in *reconnectCellId* in *VarRLF-Report* to the global cell identity and the tracking area code of the PCell;

1> if the UE supports RLF report for inter-RAT MRO NR as defined in TS 36.306 [62], and if the UE has radio link failure or handover failure information available in *VarRLF-Report* of TS 36.331 [10] and if the RPLMN is included in *plmn-IdentityList* stored in *VarRLF-Report* of TS 36.331 [10]:

2> if *reconnectCellId* in *VarRLF-Report* of TS 36.331[10] is not set after failing to perform reestablishment:

3> set *timeUntilReconnection* in *VarRLF-Report* of TS 36.331[10] to the time that elapsed since the last radio link failure or handover failure in LTE;

3> set *nrReconnectCellId* in *reconnectCellId* in *VarRLF-Report* of TS 36.331[10] to the global cell identity and the tracking area code of the PCell;

1> set the content of *RRCSetupComplete* message as follows:

2> if upper layers provide a 5G-S-TMSI:

3> if the *RRCSetup* is received in response to an *RRCSetupRequest*:

4> set the *ng-5G-S-TMSI-Value* to *ng-5G-S-TMSI-Part2*;

3> else:

4> set the *ng-5G-S-TMSI-Value* to *ng-5G-S-TMSI*;

2> if upper layers selected an SNPN or a PLMN and in case of PLMN UE is either allowed or instructed to access the PLMN via a cell for which at least one CAG ID is broadcast:

3> set the *selectedPLMN-Identity* from the *npn-IdentityInfoList*;

2> else:

3> set the *selectedPLMN-Identity* to the PLMN selected by upper layers from the *plmn-IdentityInfoList*;

2> if upper layers provide the 'Registered AMF':

3> include and set the *registeredAMF* as follows:

4> if the PLMN identity of the 'Registered AMF' is different from the PLMN selected by the upper layers:

5> include the *plmnIdentity* in the *registeredAMF* and set it to the value of the PLMN identity in the 'Registered AMF' received from upper layers;

4> set the *amf-Identifier* to the value received from upper layers;

3> include and set the *guami-Type* to the value provided by the upper layers;

2> if upper layers provide one or more S-NSSAI (see TS 23.003 [21]):

3> include the *s-NSSAI-List* and set the content to the values provided by the upper layers;

2> if upper layers provide onboarding request indication:

3> include the *onboardingRequest*;

2> set the *dedicatedNAS-Message* to include the information received from upper layers;

2> if connecting as an IAB-node:

3> include the *iab-NodeIndication*;

2> if the SIB1 contains *idleModeMeasurementsNR* and the UE has NR idle/inactive measurement information concerning cells other than the PCell available in *VarMeasIdleReport*; or

2> if the SIB1 contains *idleModeMeasurementsEUTRA* and the UE has E-UTRA idle/inactive measurement information available in *VarMeasIdleReport*:

3> include the *idleMeasAvailable*;

2> if the SIB1 contains *idleModeFR2-MeasurementsNR* and the UE is configured with*VarMeasIdleConfig-r18*:

3> include and set *fr2-MeasAvailable* in accordance with 5.7.8.5;

2> if the UE has logged measurements available for NR and if the RPLMN is included in *plmn-IdentityList* stored in *VarLogMeasReport*:

3> include the *logMeasAvailable* in the *RRCSetupComplete* message;

3> if Bluetooth measurement results are included in the logged measurements the UE has available for NR:

4> include the *logMeasAvailableBT* in the *RRCSetupComplete* message;

3> if WLAN measurement results are included in the logged measurements the UE has available for NR:

4> include the *logMeasAvailableWLAN* in the *RRCSetupComplete* message;

2> if the *sigLoggedMeasType* in *VarLogMeasReport* is included:

3> if T330 timer is running and the logged measurements configuration is for NR:

4> set *sigLogMeasConfigAvailable* to *true* in the *RRCSetupComplete* message;

3> else:

4> if the UE has logged measurements available for NR:

5> set *sigLogMeasConfigAvailable* to *false* in the *RRCSetupComplete* message;

2> if the UE has connection establishment failure or connection resume failure information available in *VarConnEstFailReport* or *VarConnEstFailReportList* and if the RPLMN is equal to *plmn-Identity* stored in *VarConnEstFailReport* or in at least one of the entries of *VarConnEstFailReportList*:

3> include *connEstFailInfoAvailable* in the *RRCSetupComplete* message;

2> if the UE has radio link failure or handover failure information available in *VarRLF-Report* and if the RPLMN is included in *plmn-IdentityList* stored in *VarRLF-Report*, or

2> if the UE has radio link failure or handover failure information available in *VarRLF-Report* of TS 36.331 [10], and if the UE is capable of cross-RAT RLF reporting and if the RPLMN is included in *plmn-IdentityList* stored in *VarRLF-Report* of TS 36.331 [10]:

3> include *rlf-InfoAvailable* in the *RRCSetupComplete* message;

2> if the UE has successful handover information available in *VarSuccessHO-Report* and if the RPLMN is included in *plmn-IdentityList* stored in *VarSuccessHO-Report*:

3> include *successHO-InfoAvailable* in the *RRCSetupComplete* message;

2> if the UE supports storage of mobility history information and the UE has mobility history information available in *VarMobilityHistoryReport*:

3> include the *mobilityHistoryAvail* in the *RRCSetupComplete* message;

2> if the UE supports uplink RRC message segmentation of *UECapabilityInformation*:

3> may include the *ul-RRC-Segmentation* in the *RRCSetupComplete* message;

2> if the *RRCSetup* is received in response to an *RRCResumeRequest*, *RRCResumeRequest1* or *RRCSetupRequest*:

3> if *speedStateReselectionPars* is configured in the *SIB2*:

4> include the *mobilityState* in the *RRCSetupComplete* message and set it to the mobility state (as specified in TS 38.304 [20]) of the UE just prior to entering RRC\_CONNECTED state;

1> submit the *RRCSetupComplete* message to lower layers for transmission, upon which the procedure ends.

*Next Modified Subclause*

5.3.8.3 Reception of the *RRCRelease* by the UE

The UE shall:

1> delay the following actions defined in this clause 60 ms from the moment the *RRCRelease* message was received or optionally when lower layers indicate that the receipt of the *RRCRelease* message has been successfully acknowledged, whichever is earlier;

1> stop timer T380, if running;

1> stop timer T320, if running;

1> if timer T316 is running;

2> stop timer T316;

2> clear the information included in *VarRLF-Report,* if any;

1> stop timer T350, if running;

1> stop timer T346g, if running;

1> if theAS security is not activated:

2> ignore any field included in *RRCRelease* message except *waitTime*;

2> perform the actions upon going to RRC\_IDLE as specified in 5.3.11 with the release cause 'other' upon which the procedure ends;

1> if the *RRCRelease* message includes *redirectedCarrierInfo* indicating redirection to *eutra*:

2> if *cnType* is included:

3> after the cell selection, indicate the available CN Type(s) and the received *cnType* to upper layers;

NOTE 1: Handling the case if the E-UTRA cell selected after the redirection does not support the core network type specified by the *cnType,* is up to UE implementation.

2> if *voiceFallbackIndication* is included:

3> consider the RRC connection release was for EPS fallback for IMS voice (see TS 23.502 [43]);

1> if the *RRCRelease* message includes the *cellReselectionPriorities*:

2> store the cell reselection priority information provided by the *cellReselectionPriorities*;

2> if the *t320* is included:

3> start timer T320, with the timer value set according to the value of *t320*;

1> else:

2> apply the cell reselection priority information broadcast in the system information;

1> if *deprioritisationReq* is included and the UE supports RRC connection release with deprioritisation:

2> start or restart timer T325 with the timer value set to the *deprioritisationTimer* signalled;

2> store the *deprioritisationReq* until T325 expiry;

NOTE 1a: The UE stores the deprioritisation request irrespective of any cell reselection absolute priority assignments (by dedicated or common signalling) and regardless of RRC connections in NR or other RATs unless specified otherwise.

1> if the *RRCRelease* includes the *measIdleConfig-r16*:

2> if T331 is running:

3> stop timer T331;

3> perform the actions as specified in 5.7.8.3;

2> if the *measIdleConfig* is set to *setup*:

3> store the received *measIdleDuration* in *VarMeasIdleConfig*;

3> start timer T331 with the value set to *measIdleDuration*;

3> if the *measIdleConfig* contains *measIdleCarrierListNR*:

4> store the received *measIdleCarrierListNR* in *VarMeasIdleConfig*;

3> if the *measIdleConfig* contains *measIdleCarrierListEUTRA*:

4> store the received *measIdleCarrierListEUTRA* in *VarMeasIdleConfig*;

3> if the *measIdleConfig* contains *validityAreaList*:

4> store the received *validityAreaList* in *VarMeasIdleConfig*;

1> if the *RRCRelease* includes the *measIdleConfig-r18*:

2> if the *measIdleConfig-r18* is set to *setup*

3> if the measIdleConfig-r18 contains measIdleFR2-CarrierNR:

4> store the received *measIdleFR2-CarrierNR* in *VarMeasIdleConfig*;

1> if the *RRCRelease* includes *suspendConfig*:

2> reset MAC and release the default MAC Cell Group configuration, if any;

2> apply the received *suspendConfig* except the received *nextHopChainingCount*;

2> if the *sdt-Config* is configured:

3> for each of the DRB in the *sdt-DRB-List*:

4> consider the DRB to be configured for SDT;

3> if *sdt-SRB2-Indication* is configured:

4> consider the SRB2 to be configured for SDT;

3> for each RLC bearer (except those associated with broadcast MRBs) that is not suspended:

4> re-establish the RLC entity as specified in TS 38.322 [4];

3> for SRB2 (if it is resumed) and for SRB1:

4> trigger the PDCP entity to perform SDU discard as specified in TS 38.323 [5];

3> if *sdt-MAC-PHY-CG-Config* is configured:

4> configure the PCell with the configured grant resources for SDT and instruct the MAC entity to start the *cg-SDT-TimeAlignmentTimer*;

2> if *srs-PosRRC-Inactive* is configured:

3> apply the configuration and instruct MAC to start the *inactivePosSRS-TimeAlignmentTimer*;

NOTE 1b: The Network should provide full configuration to UE for SRS for Positioning in RRC\_INACTIVE.

2> remove all the entries within the MCG and the SCG *VarConditionalReconfig*, if any;

2> for each *measId* of the MCG *measConfig* and for each *measId* of the SCG *measConfig*, if configured, if the associated *reportConfig* has a *reportType* set to *condTriggerConfig*:

3> for the associated *reportConfigId*:

4> remove the entry with the matching *reportConfigId* from the *reportConfigList* within the *VarMeasConfig*;

3> if the associated *measObjectId* is only associated to a *reportConfig* with *reportType* set to *condTriggerConfig*:

4> remove the entry with the matching *measObjectId* from the *measObjectList* within the *VarMeasConfig*;

3> remove the entry with the matching *measId* from the *measIdList* within the *VarMeasConfig*;

2> if the UE is acting as L2 U2N Remote UE:

3> if the PC5-RRC connection with the U2N Relay UE is determined to be released:

4> indicate upper layers to trigger PC5 unicast link release;

3> else (i.e., maintain the PC5 RRC connection):

4> establish or re-establish (e.g. via release and add) SL RLC entity for SRB1;

2> else:

3> re-establish RLC entities for SRB1;

2> if the *RRCRelease* message with *suspendConfig* was received in response to an *RRCResumeRequest* or an *RRCResumeRequest1*:

3> stop the timer T319 if running;

3> in the stored UE Inactive AS context:

4> replace the KgNB and KRRCint keys with the current KgNB and KRRCint keys;

4> replace the *nextHopChainingCount* with the value of *nextHopChainingCount* received in the *RRCRelease* message*;*

4> replace the *cellIdentity* with the *cellIdentity* of the cell the UE has received the *RRCRelease* message;

4> if the *suspendConfig* contains the *sl-UEIdentityRemote* (i.e. the UE is a L2 U2N Remote UE):

5> replace the C-RNTI with the value of the *sl-UEIdentityRemote*;

5> replace the physical cell identitywith the value of the *sl-PhysCellId* in *sl-ServingCellInfo* contained in the discovery message received from the connected L2 U2N Relay UE;

4> else:

5> replace the C-RNTI with the C-RNTI used in the cell (see TS 38.321 [3]) the UE has received the *RRCRelease* message;

5> replace the physical cell identitywith the physical cell identity of the cell the UE has received the *RRCRelease* message;

3> replace the *nextHopChainingCount* with the value associated with the current KgNB;

3> stop the timer T319a if running and consider SDT procedure is not ongoing;

2> else:

3> store in the UE Inactive AS Context the *nextHopChainingCount* received in the *RRCRelease* message*,* the current KgNB and KRRCint keys, the ROHC state, the EHC context(s), the UDC state, the stored QoS flow to DRB mapping rules, the application layer measurement configuration, the C-RNTI used in the source PCell, the *cellIdentity* and the physical cell identity of the source PCell, the *spCellConfigCommon* within *ReconfigurationWithSync* of the NR PSCell (if configured) and all other parameters configured except for:

- parameters within *ReconfigurationWithSync* of the PCell;

- parameters within *ReconfigurationWithSync* of the NR PSCell, if configured;

- parameters within *MobilityControlInfoSCG* of the E-UTRA PSCell, if configured;

- *servingCellConfigCommonSIB*;

- *sl-L2RelayUE-Config*, if configured;

- *sl-L2RemoteUE-Config*, if configured;

NOTE 1c: *suspendConfig* is not stored as part of UE Inactive AS Context, except for the fields explicitly specified.

3> store any previously or subsequently received application layer measurement report containers for which no segment, or full message, has been submitted to lower layers for transmission;

NOTE 2: NR sidelink communication/discovery related configurations and logged measurement configuration are not stored as UE Inactive AS Context, when UE enters RRC\_INACTIVE.

2> suspend all SRB(s) and DRB(s) and multicast MRB(s), except SRB0 and broadcast MRBs;

2> indicate PDCP suspend to lower layers of all DRBs and multicast MRBs;

2> release Uu Relay RLC channel(s), if configured;

2> release PC5 Relay RLC channel(s), if configured;

2> release the SRAP entity, if configured;

2> if the *t380* is included:

3> start timer T380, with the timer value set to *t380*;

2> if the *RRCRelease* message is including the *waitTime*:

3> start timer T302 with the value set to the *waitTime*;

3> inform upper layers that access barring is applicable for all access categories except categories '0' and '2';

2> if T390 is running:

3> stop timer T390 for all access categories;

3> perform the actions as specified in 5.3.14.4;

2> indicate the suspension of the RRC connection to upper layers;

2> if the UE is capable of L2 U2N Remote UE:

3> enter RRC\_INACTIVE, and perform either cell selection as specified in TS 38.304 [20], or relay selection as specified in clause 5.8.15.3, or both;

2> else:

3> enter RRC\_INACTIVE and perform cell selection as specified in TS 38.304 [20];

1> else:

2> perform the actions upon going to RRC\_IDLE as specified in 5.3.11, with the release cause 'other'.

NOTE 3: Whether to release the PC5 unicast link is left to L2 U2N Remote UE's implementation.

NOTE 4: It is left to UE implementation whether to stop T430, if running, when going to RRC\_INACTIVE.

*Next Modified Subclause*

5.3.13.4 Reception of the *RRCResume* by the UE

The UE shall:

1> stop timer T319, if running;

1> stop timer T319a, if running and consider SDT procedure is not ongoing;

1> stop timer T380, if running;

1> if T331 is running:

2> stop timer T331;

2> perform the actions as specified in 5.7.8.3;

1> if the *RRCResume* includes the *fullConfig*:

2> perform the full configuration procedure as specified in 5.3.5.11;

1> else:

2> if the *RRCResume* does not include the *restoreMCG-SCells*:

3> release the MCG SCell(s) from the UE Inactive AS context, if stored;

2> if the *RRCResume* does not include the *restoreSCG*:

3> release the MR-DC related configurations (i.e., as specified in 5.3.5.10) from the UE Inactive AS context, if stored;

2> restore the *masterCellGroup, mrdc-SecondaryCellGroup*, if stored, and *pdcp-Config* from the UE Inactive AS context;

2> configure lower layers to consider the restored MCG and SCG SCell(s) (if any) to be in deactivated state;

1> discard the UE Inactive AS context;

1> store the used *nextHopChainingCount* value associated to the current KgNB;

1> if *sdt-MAC-PHY-CG-Config* is configured:

2> instruct the MAC entity to stop the *cg-SDT-TimeAlignmentTimer*, if it is running;

2> instruct the MAC entity to start the *timeAlignmentTimer* associated with the PTAG*,* if it is not running;

1> if *srs-PosRRC-InactiveConfig* is configured:

2> instruct the MAC entity to stop *inactivePosSRS-TimeAlignmentTimer*, if it is running;

1> release the *suspendConfig* except the *ran-NotificationAreaInfo*;

1> if the *RRCResume* includes the *masterCellGroup*:

2> perform the cell group configuration for the received *masterCellGroup* according to 5.3.5.5;

1> if the *RRCResume* includes the *mrdc-SecondaryCellGroup:*

2> if the received *mrdc-SecondaryCellGroup* is set to *nr-SCG*:

3> perform the RRC reconfiguration according to 5.3.5.3 for the *RRCReconfiguration* message included in *nr-SCG*;

2> if the received *mrdc-SecondaryCellGroup* is set to *eutra-SCG*:

3> perform the RRC connection reconfiguration as specified in TS 36.331 [10], clause 5.3.5.3 for the *RRCConnectionReconfiguration* message included in *eutra-SCG*;

1> if the *RRCResume* includes the *radioBearerConfig*:

2> perform the radio bearer configuration according to 5.3.5.6;

1> if the *RRCResume* message includes the *sk-Counter*:

2> perform security key update procedure as specified in 5.3.5.7;

1> if the *RRCResume* message includes the *radioBearerConfig2*:

2> perform the radio bearer configuration according to 5.3.5.6;

1> if the *RRCResume* message includes the *needForGapsConfigNR*:

2> if *needForGapsConfigNR* is set to *setup*:

3> consider itself to be configured to provide the measurement gap requirement information of NR target bands;

2> else:

3> consider itself not to be configured to provide the measurement gap requirement information of NR target bands;

1> if the *RRCResume* message includes the *needForGapNCSG-ConfigNR*:

2> if *needForGapNCSG-ConfigNR* is set to *setup*:

3> consider itself to be configured to provide the measurement gap and NCSG requirement information of NR target bands;

2> else:

3> consider itself not to be configured to provide the measurement gap and NCSG requirement information of NR target bands;

1> if the *RRCResume* message includes the *needForGapNCSG-ConfigEUTRA*:

2> if *needForGapNCSG-ConfigEUTRA* is set to *setup*:

3> consider itself to be configured to provide the measurement gap and NCSG requirement information of E‑UTRA target bands;

2> else:

3> consider itself not to be configured to provide the measurement gap and NCSG requirement information of E‑UTRA target bands;

1> if the *RRCResume* message includes the *appLayerMeasConfig*:

2> perform the application layer measurement configuration procedure as specified in 5.3.5.13d;

1> if the *RRCResume* message includes the *sl-L2RemoteUE-Config* (i.e. the UE is a L2 U2N Remote UE):

2> perform the L2 U2N Remote UE configuration procedure as specified in 5.3.5.16;

1> if the *RRCResume* message includes the *sl-ConfigDedicatedNR*:

2> perform the sidelink dedicated configuration procedure as specified in 5.3.5.14;

1> resume SRB2 (if suspended), SRB3 (if configured), SRB4 (if configured), all DRBs (that are suspended) and multicast MRBs;

NOTE 1: If the SCG is deactivated, resuming SRB3 and all DRBs does not imply that PDCP or RRC PDUs can be transmitted or received on SCG RLC bearers.

1> if stored, discard the cell reselection priority information provided by the *cellReselectionPriorities* or inherited from another RAT;

1> stop timer T320, if running;

1> if the *RRCResume* message includes the *measConfig*:

2> perform the measurement configuration procedure as specified in 5.5.2;

1> resume measurements if suspended;

1> if T390 is running:

2> stop timer T390 for all access categories;

2> perform the actions as specified in 5.3.14.4;

1> if T302 is running:

2> stop timer T302;

2> perform the actions as specified in 5.3.14.4;

1> enter RRC\_CONNECTED;

1> indicate to upper layers that the suspended RRC connection has been resumed;

1> stop the cell re-selection procedure;

1> stop relay reselection procedure if any for L2 U2N Remote UE;

1> consider the current cell to be the PCell;

1> set the content of the of *RRCResumeComplete* message as follows:

2> if the upper layer provides NAS PDU, set the *dedicatedNAS-Message* to include the information received from upper layers;

2> if upper layers provides a PLMN:

3> if the UE is either allowed or instructed to access the PLMN via a cell for which at least one CAG ID is broadcast:

4> set the *selectedPLMN-Identity* from the *npn-IdentityInfoList*;

3> else:

4> set the *selectedPLMN-Identity* to the PLMN selected by upper layers from the *plmn-IdentityInfoList*;

2> if the *masterCellGroup* contains the *reportUplinkTxDirectCurrent*:

3> include the *uplinkTxDirectCurrentList* for each MCG serving cell with UL;

3> include *uplinkDirectCurrentBWP-SUL* for each MCG serving cell configured with SUL carrier, if any, within the *uplinkTxDirectCurrentList*;

2> if the *masterCellGroup* contains the *reportUplinkTxDirectCurrentTwoCarrier*:

3> include in the *uplinkTxDirectCurrentTwoCarrierList* the list of uplink Tx DC locations for the configured uplink carrier aggregation in the MCG;

2> if the *masterCellGroup* contains the *reportUplinkTxDirectCurrentMoreCarrier*:

3> include in the *uplinkTxDirectCurrentMoreCarrierList* the list of uplink Tx DC locations for the configured uplink carrier aggregation in the MCG;

2> if the UE has idle/inactive measurement information concerning cells other than the PCell available in *VarMeasIdleReport*:

3> if the *idleModeMeasurementReq* is included in the *RRCResume* message:

4> set the *measResultIdleEUTRA* in the *RRCResumeComplete* message to the value of *measReportIdleEUTRA* in the *VarMeasIdleReport,* if available;

4> set the *measResultIdleNR* in the *RRCResumeComplete* message to the value of *measReportIdleNR* in the *VarMeasIdleReport*, if available;

4> discard the *VarMeasIdleReport* upon successful delivery of the *RRCResumeComplete* message is confirmed by lower layers;

3> else:

4> if the SIB1 contains *idleModeMeasurementsNR* and the UE has NR idle/inactive measurement information concerning cells other than the PCell available in *VarMeasIdleReport*; or

4> if the SIB1 contains *idleModeMeasurementsEUTRA* and the UE has E-UTRA idle/inactive measurement information available in *VarMeasIdleReport*:

5> include the *idleMeasAvailable*;

2> if the UE is configured with *VarMeasIdleConfig-r18:*

3> if the *fr2*-*idleModeMeasurementReq* is included in the *RRCResume* message:

4> set the *measResultIdleFR2-NR* in the *RRCResumeComplete* message to the value of *measReportIdleFR2-NR* in the *VarMeasIdleReport-r18*, if available;

4> discard the *VarMeasIdleReport-r18* upon successful delivery of the *RRCResumeComplete* message is confirmed by lower layers;

3> else:

4> if the SIB1 contains *idleModeMeasurementsNR* and the UE has NR FR2 idle/inactive measurement information concerning cells other than the PCell available in *VarMeasIdleReport-r18*; or

5> include the *fr2-MeasAvailable* in accordance with 5.7.8.5;

2> if the *RRCResume* message includes *mrdc-SecondaryCellGroup* set to *eutra-SCG*:

3> include in the *eutra-SCG-Response* the E-UTRA *RRCConnectionReconfigurationComplete* message in accordance with TS 36.331 [10] clause 5.3.5.3;

2> if the *RRCResume* message includes *mrdc-SecondaryCellGroup* set to *nr-SCG*:

3> include in the *nr-SCG-Response* the SCG *RRCReconfigurationComplete* message;

2> if the UE has logged measurements available for NR and if the RPLMN is included in *plmn-IdentityList* stored in *VarLogMeasReport*:

3> include the *logMeasAvailable* in the *RRCResumeComplete* message*;*

3> if Bluetooth measurement results are included in the logged measurements the UE has available for NR:

4> include the *logMeasAvailableBT* in the *RRCResumeComplete* message;

3> if WLAN measurement results are included in the logged measurements the UE has available for NR:

4> include the *logMeasAvailableWLAN* in the *RRCResumeComplete* message;

2> if the *sigLoggedMeasType* in *VarLogMeasReport* is included:

3> if T330 timer is running and the logged measurements configuration is for NR:

4> set *sigLogMeasConfigAvailable* to *true* in the *RRCResumeComplete* message;

3> else:

4> if the UE has logged measurements available for NR:

5> set *sigLogMeasConfigAvailable* to *false* in the *RRCResumeComplete* message;

2> if the UE has connection establishment failure or connection resume failure information available in *VarConnEstFailReport* or *VarConnEstFailReportList* and if the RPLMN is equal to *plmn-Identity* stored in *VarConnEstFailReport* orin at least one of the entries of *VarConnEstFailReportList*:

3> include *connEstFailInfoAvailable* in the *RRCResumeComplete* message;

2> if the UE has radio link failure or handover failure information available in *VarRLF-Report* and if the RPLMN is included in *plmn-IdentityList* stored in *VarRLF-Report*; or

2> if the UE has radio link failure or handover failure information available in *VarRLF-Report* of TS 36.331 [10] and if the UE is capable of cross-RAT RLF reporting and if the RPLMN is included in *plmn-IdentityList* stored in *VarRLF-Report* of TS 36.331 [10]:

3> include *rlf-InfoAvailable* in the *RRCResumeComplete* message;

2> if the UE has successful handover information available in *VarSuccessHO-Report* and if the RPLMN is included in *plmn-IdentityList* stored in *VarSuccessHO-Report*:

3> include *successHO-InfoAvailable* in the *RRCResumeComplete* message;

2> if the UE supports storage of mobility history information and the UE has mobility history information available in *VarMobilityHistoryReport*:

3> include the *mobilityHistoryAvail* in the *RRCResumeComplete* message;

2> if *speedStateReselectionPars* is configured in the *SIB2*:

3> include the *mobilityState* in the *RRCResumeComplete* message and set it to the mobility state (as specified in TS 38.304 [20]) of the UE just prior to entering RRC\_CONNECTED state;

2> if the UE is configured to provide the measurement gap requirement information of NR target bands:

3> include the *NeedForGapsInfoNR* and set the contents as follows:

4> include *intraFreq-needForGap* and set the gap requirement information of intra-frequency measurement for each NR serving cell;

4> if *requestedTargetBandFilterNR* is configured, for each supported NR band that is also included in *requestedTargetBandFilterNR*, include an entry in *interFreq-needForGap* and set the gap requirement information for that band; otherwise, include an entry in *interFreq-needForGap* and set the corresponding gap requirement information for each supported NR band;

2> if the UE is configured to provide the measurement gap and NCSG requirement information of NR target bands:

3> include the *NeedForGapNCSG-InfoNR* and set the contents as follows:

4> include *intraFreq-needForNCSG* and set the gap and NCSG requirement information of intra-frequency measurement for each NR serving cell;

4> if *requestedTargetBandFilterNCSG-NR* is configured:

5> for each supported NR band included in *requestedTargetBandFilterNCSG-NR*, include an entry in *interFreq-needForNCSG* and set the NCSG requirement information for that band;

4> else:

5> include an entry for each supported NR band in *interFreq-needForNCSG* and set the corresponding NCSG requirement information;

2> if the UE is configured to provide the measurement gap and NCSG requirement information of E‑UTRA target bands:

3> include the *NeedForGapNCSG-InfoEUTRA* and set the contents as follows:

4> if *requestedTargetBandFilterNCSG-EUTRA* is configured:

5> for each supported E-UTRA band included in *requestedTargetBandFilterNCSG-EUTRA*, include an entry in *needForNCSG-EUTRA* and set the NCSG requirement information for that band;

4> else:

5> include an entry for each supported E-UTRA band in *needForNCSG-EUTRA* and set the corresponding NCSG requirement information;

1> submit the *RRCResumeComplete* message to lower layers for transmission;

1> the procedure ends.

NOTE 2: Network only configures at most one of *reportUplinkTxDirectCurrent, reportUplinkTxDirectCurrentTwoCarrier* or *reportUplinkTxDirectCurrentMoreCarrier* in one RRC message*.*

*Next Modified Subclause*

5.7.8.1b FR2 Measurement configuration

The purpose of this procedure is to update the FR2 idle/inactive measurement configuration.

The UE initiates this procedure while *varMeasIdleConfig-r18*  is configured and SDT procedure is not ongoing and one of the following conditions is met:

1> upon selecting a cell when entering RRC\_IDLE or RRC-INACTIVE from RRC\_CONNECTED or RRC\_INACTIVE; or

1> upon update of system information (*SIB11*), e.g. due to intra-RAT cell (re)selection;

While in RRC\_IDLE or RRC\_INACTIVE and *varMeasIdleConfig-r18* is configured, the UE shall:

1> if *VarMeasIdleConfig-r18* includes *measIdleFR2-CarrierNR* received from the *RRCRelease* message:

2> if the UE supports *idleInactiveFR2-NR-MeasReport*:

3> if *SIB11* includes the *measIdleConfigSIB* and contains *measIdleFR2-CarrierNR*:

4> store or replace the *measIdleFR2-CarrierNR* of *measIdleConfigSIB* of *SIB11* within *VarMeasIdleConfig*;

3> else:

4> remove the *measIdleFR2-CarrierNR* in *VarMeasIdleConfig*, if stored;

1>if *measIdleFR2-CarrierNR* within *VarMeasIdleConfig* does not contain an *ssb-MeasConfig* received from the *RRCRelease* message:

2> if there is an entry in *measIdleFR2-CarrierNR* in *measIdleConfigSIB* of *SIB11* that has the same carrier frequency and subcarrier spacing as the entry in the *measIdleFR2-CarriertNR* within *VarMeasIdleConfig* and that contains *ssb-MeasConfig*:

3> delete the *ssb-MeasConfig* of the corresponding entry in the *measIdleCarrierListNR* within *VarMeasIdleConfig*;

3> store the SSB measurement configuration from *SIB11* into *nrofSS-BlocksToAverage*, *absThreshSS-BlocksConsolidation*, *smtc*, *ssb-ToMeasure*, *deriveSSB-IndexFromCell*, and *ss-RSSI-Measurement* within *ssb-MeasConfig* in the *measIdleFR2-CarrierNR* within *VarMeasIdleConfig*;

2> else if there is an entry in *interFreqCarrierFreqList* of *SIB4* with the same carrier frequency and subcarrier spacing as the entry in *measIdleFR2-CarriertNR* within *VarMeasIdleConfig*:

3> delete the *ssb-MeasConfig* in the *measIdleFR2-CarrierNR* within *VarMeasIdleConfig*;

3> store the SSB measurement configuration from *SIB4* into *nrofSS-BlocksToAverage*, *absThreshSS-BlocksConsolidation*, *smtc*, *ssb-ToMeasure*, *deriveSSB-IndexFromCell*, and *ss-RSSI-Measurement* within *ssb-MeasConfig* of the corresponding entry in the *measIdleFR2-CarrierNR* within *VarMeasIdleConfig*;

2> else:

3> remove the *ssb-MeasConfig* of the corresponding entry in the *measIdleFR2-CarrierNR* within *VarMeasIdleConfig*, if stored;

1> perform measurements according to 5.7.8.2b.

*Next Modified Subclause*

5.7.8.2b Performing FR2 measurements during RRC connection setup/resume

While SDT procedure is not ongoing, the UE shall:

1> perform the measurements in accordance with the following:

2> if the *VarMeasIdleConfig-r18* includes the *measIdleFR2-CarrierNR-r18*:

3> for each entry in *measIdleFR2-CarrierNR* within *VarMeasIdleConfig-r18* that contains *ssb-MeasConfig*:

4> if UE supports carrier aggregation or NR-DC between serving carrier and the carrier frequency and subcarrier spacing indicated by *carrierFreq* and *ssbSubCarrierSpacing* within the corresponding entry:

5> perform measurements in the carrier frequency and subcarrier spacing indicated by *carrierFreq* and *ssbSubCarrierSpacing* within the corresponding entry;

5> if the *reportQuantities* is set to rsrq:

6> consider RSRQ as the cell sorting quantity;

5> else:

6> consider RSRP as the cell sorting quantity;

5> if the *measCellListNR* is included:

6> consider cells identified by each entry within the *measCellListNR* to be applicable for idle/inactive measurement reporting;

5> else:

6> consider up to *maxCellMeasIdleFR2* strongest identified cells, according to the sorting quantity, to be applicable for idle/inactive measurement reporting;

5> for all cells applicable for idle/inactive measurement reporting, derive cell measurement results for the measurement quantities indicated by *reportQuantities;*

5> store the derived cell measurement results as indicated by *reportQuantities* for cells applicable for idle/inactive measurement reporting within *measResultsPerCarrierListIdleNR* in the *measReportIdleNR* in *VarMeasIdleReport-r18* in decreasing order of the cell sorting quantity, i.e. the best cell is included first, as follows:

6> if *qualityThreshold* is configured:

7> include the measurement results from the cells applicable for idle/inactive measurement reporting whose RSRP/RSRQ measurement results are above the value(s) provided in *qualityThreshold;*

6> else:

7> include the measurement results from all cells applicable for idle/inactive measurement reporting;

5> if *beamMeasConfigIdle* is included in the associated entry in *measIdleCarrierListNR*, for each cell in the measurement results:

6> derive beam measurements based on SS/PBCH block for each measurement quantity indicated in *reportQuantityRS-Indexes*, as described in TS 38.215 [9];

6> if the *reportQuantityRS-Indexes* is set to rsrq:

7> consider RSRQ as the beam sorting quantity;

6> else:

7> consider RSRP as the beam sorting quantity;

6> set *resultsSSB-Indexes* to include up to *maxNrofRS-IndexesToReport* SS/PBCH block indexes in order of decreasing beam sorting quantity as follows:

7> include the index associated to the best beam for the sorting quantity and if *absThreshSS-BlocksConsolidation* is included, the remaining beams whose sorting quantity is above *absThreshSS-BlocksConsolidation*;

6> if the *includeBeamMeasurements* is set to *true*:

7> include the beam measurement results as indicated by *reportQuantityRS*-*Indexes*;

2> if, as a result of the procedure in this clause, the UE performs measurements indicated by *measIdleFR2-CarrierNR*:

3> store the cell measurement results for RSRP and RSRQ for the serving cell within *measResultServingCell* in the *measReportIdleNR* in *VarMeasIdleReport-r18*.

3> if the *VarMeasIdleConfig-r18* includes the *measIdleFR2-CarrierNR* and it contains an entry with *carrierFreq* set to the value of the serving frequency:

4> if *beamMeasConfigIdle* is included in that entry:

5> derive beam measurements based on SS/PBCH block for each measurement quantity indicated in *reportQuantityRS-Indexes*, as described in TS 38.215 [9];

5> if the *reportQuantityRS-Indexes* is set to rsrq:

6> consider RSRQ as the beam sorting quantity;

5> else:

6> consider RSRP as the beam sorting quantity;

5> set *resultsSSB-Indexes* to include up to *maxNrofRS-IndexesToReport* SS/PBCH block indexes in order of decreasing beam sorting quantity as follows:

6> include the index associated to the best beam for the sorting quantity and if *absThreshSS-BlocksConsolidation* is included in *SIB2* of serving cell, the remaining beams whose sorting quantity is above *absThreshSS-BlocksConsolidation*;

5> if the *includeBeamMeasurements* is set to true:

6> include the beam measurement results as indicated by *reportQuantityRS-Indexes*;

*Next Modified Subclause*

5.7.8.4b Cell re-selection or cell selection while FR2 measurements are configured

The UE shall:

1> if inter-RAT cell selection or reselection occurs while UE is configured with *VarMeasIdleConfig-r18*:

2> release the *VarMeasIdleConfig-r18;*

5.7.8.5 Availability of the measurements

2> if UE has, as defined in 38.133[] clause x.y.z, available results for the the carrier frequency and subcarrier spacing indicated by *carrierFreq* and *ssbSubCarrierSpacing* within in *VarMeasIdleReport-r18*:

3> set the value *fr2-MeasAvailable* for the the corresponding entry in *VarMeasIdleReport-r18* as *available;*

2> else

3> set the value *fr2-MeasAvailable* for the the corresponding entry in *VarMeasIdleReport-r18* as *ongoing;*

*Next Modified Subclause*

5.7.10 UE Information

5.7.10.1 General

****

**Figure 5.7.10.1-1: UE information procedure**

The UE information procedure is used by the network to request the UE to report information.

5.7.10.2 Initiation

The network initiates the procedure by sending the *UEInformationRequest* message. The network should initiate this procedure only after successful security activation.

5.7.10.3 Reception of the *UEInformationRequest* message

Upon receiving the *UEInformationRequest* message, the UE shall, only after successful security activation:

1> if the *idleModeMeasurementReq* is included in the *UEInformationRequest* and the UE has stored *VarMeasIdleReport* that contains measurement information concerning cells other than the PCell:

2> set the *measResultIdleEUTRA* in the *UEInformationResponse* message to the value of *measReportIdleEUTRA* in the *VarMeasIdleReport, if available*;

2> set the *measResultIdleNR* in the *UEInformationResponse* message to the value of *measReportIdleNR* in the *VarMeasIdleReport*, if available;

2> discard the *VarMeasIdleReport* upon successful delivery of the *UEInformationResponse* message confirmed by lower layers;

1> if the *fr2-MeasurementReq* is included in the *UEInformationRequest* and the UE has stored *VarMeasIdleReport-r18* that contains measurement information concerning cells other than the PCell:

2> set the *measResultIdleNR-r18* in the *UEInformationResponse* message to the value of *measReportIdleNR* in the *VarMeasIdleReport-r18*, if available;

2> discard the *VarMeasIdleReport-r18* upon successful delivery of the *UEInformationResponse* message confirmed by lower layers;

1> if the *logMeasReportReq* is present and if the RPLMN is included in *plmn-IdentityList* stored in *VarLogMeasReport*:

2> if *VarLogMeasReport* includes one or more logged measurement entries, set the contents of the *logMeasReport* in the *UEInformationResponse* message as follows:

3> include the *absoluteTimeStamp* and set it to the value of *absoluteTimeInfo* in the *VarLogMeasReport*;

3> include the *traceReference* and set it to the value of *traceReference* in the *VarLogMeasReport*;

3> include the *traceRecordingSessionRef* and set it to the value of *traceRecordingSessionRef* in the *VarLogMeasReport;*

3> include the *tce-Id* and set it to the value of *tce-Id* in the *VarLogMeasReport*;

3> include the *logMeasInfoList* and set it to include one or more entries from the *VarLogMeasReport* starting from the entries logged first, and for each entry of the *logMeasInfoList* that is included, include all information stored in the corresponding *logMeasInfoList* entry in *VarLogMeasReport*;

3> if the *VarLogMeasReport* includes one or more additional logged measurement entries that are not included in the *logMeasInfoList* within the *UEInformationResponse* message:

4> include the *logMeasAvailable*;

4> if *bt-LocationInfo* is included in *locationInfo* of one or more of the additional logged measurement entries in *VarLogMeasReport* that are not included in the *logMeasInfoList* within the *UEInformationResponse* message:

5> include the *logMeasAvailableBT*;

4> if *wlan-LocationInfo* is included in *locationInfo* of one or more of the additional logged measurement entries in *VarLogMeasReport* that are not included in the *logMeasInfoList* within the *UEInformationResponse* message:

5> include the *logMeasAvailableWLAN*;

1> if *ra-ReportReq* is set to *true* and the UE has random access related information available in *VarRA-Report* and if the RPLMN is included in *plmn-IdentityList* stored in *VarRA-Report*:

2> set the *ra-ReportList* in the *UEInformationResponse* message to the value of *ra-ReportList* in *VarRA-Report*;

2> discard the *ra-ReportList* from *VarRA-Report* upon successful delivery of the *UEInformationResponse* message confirmed by lower layers;

1> if *rlf-ReportReq* is set to *true*:

2> if the UE has radio link failure information or handover failure information available in *VarRLF-Report* and if the RPLMN is included in *plmn-IdentityList* stored in *VarRLF-Report*:

3> set *timeSinceFailure* in *VarRLF-Report* to the time that elapsed since the last radio link failure or handover failure in NR;

3> set the *rlf-Report* in the *UEInformationResponse* message to the value of *rlf-Report* in *VarRLF-Report*;

3> discard the *rlf-Report* from *VarRLF-Report* upon successful delivery of the *UEInformationResponse* message confirmed by lower layers;

2> else if the UE is capable of cross-RAT RLF reporting as defined in TS 38.306 [26] and has radio link failure information or handover failure information available in *VarRLF-Report* of TS 36.331 [10] and if the RPLMN is included in *plmn-IdentityList* stored in *VarRLF-Report* of TS 36.331 [10]:

3> set *timeSinceFailure* in *VarRLF-Report* of TS 36.331 [10] to the time that elapsed since the last radio link failure or handover failure in EUTRA;

3> set failedPCellId-EUTRA in the *rlf-Report* in the *UEInformationResponse* message to indicate the PCell in which RLF was detected or the source PCell of the failed handover in the *VarRLF-Report* of TS 36.331 [10];

3> set the *measResult-RLF-Report-EUTRA* in the *rlf-Report* in the *UEInformationResponse* message to the value of *rlf-Report* in *VarRLF-Report* of TS 36.331 [10];

3> discard the *rlf-Report* from *VarRLF-Report* of TS 36.331 [10] upon successful delivery of the *UEInformationResponse* message confirmed by lower layers;

1> if *connEstFailReportReq* is set to *true* and the UE has connection establishment failure or connection resume failure information in *VarConnEstFailReport* or *VarConnEstFailReportList* and if the RPLMN is equal to *plmn-Identity* stored in *VarConnEstFailReport* orin at least one of the entries of *VarConnEstFailReportList*:

2> set *timeSinceFailure* in *VarConnEstFailReport* to the time that elapsed since the last connection establishment failure or connection resume failure in NR;

2> set the *connEstFailReport* in the *UEInformationResponse* message to the value of *connEstFailReport* in *VarConnEstFailReport*;

2> if the UE supports multiple CEF report:

3> for each *connEstFailReport* in the *connEstFailReportList* in *VarConnEstFailReportList*:

4> set *timeSinceFailure* to the time that elapsed since the associated connection establishment failure or connection resume failure in NR;

2> for each *connEstFailReport* in the *connEstFailReportList* in the *UEInformationResponse* message, set the value to the value of *connEstFailReport* in *VarConnEstFailReport* in *VarConnEstFailReportList*;

2> discard the *connEstFailReport* from *VarConnEstFailReport* and *VarConnEstFailReportList* upon successful delivery of the *UEInformationResponse* message confirmed by lower layers;

1> if the *mobilityHistoryReportReq* is set to *true*:

2> include the *mobilityHistoryReport* and set it to include *visitedCellInfoList* from *VarMobilityHistoryReport*;

2> include in the *mobilityHistoryReport* an entry for the current PCell, possibly after removing the oldest entry if required, and set its fields as follows:

3> set *visitedCellId* to the global cell identity or the physical cell identity and carrier frequency of the current PCell:

3> set field *timeSpent* to the time spent in the current PCell;

3> if the UE supports PSCell mobility history information and if *visitedPSCellInfoList* is present in *VarMobilityHistoryReport*:

4> for the newest entry of the PCell in the *mobilityHistoryReport*, include *visitedPSCellInfoList* from *VarMobilityHistoryReport*;

4> if the UE is configured with a PSCell:

5> for the newest entry of the PCell in the *mobilityHistoryReport*, include the current PSCell information in the *visitedPSCellInfoListReport,* possibly after removing the oldest PSCell entry of a PCell in the *mobilityHistoryReport*, if required, and set its fields as follows:

6> set *visitedCellId* to the global cell identity or the physical cell identity and carrier frequency of the current PSCell:

6> set field *timeSpent* to the time spent in the current PSCell while being connected to the current PCell;

4> else:

5> for the newest entry of the PCell in the *mobilityHistoryReport*, include a new entry in the *visitedPSCellInfoListReport,* possibly after removing the oldest PSCell entry of a PCell in the *mobilityHistoryReport*, if required, and set its fields as follows:

6> set field *timeSpent* to the time spent without PSCell in the current PCell since last PSCell release since connected to the current PCell in RRC\_CONNECTED;

3> else if the UE supports PSCell mobility history information:

4> if the UE is configured with a PSCell:

5> for the newest entry of the PCell in the *mobilityHistoryReport*, include the current PSCell information in the *visitedPSCellInfoListReport,* possibly after removing the oldest PSCell entry of a PCell in the *mobilityHistoryReport*, if required, and set its fields as follows:

6> set *visitedCellId* to the global cell identity or the physical cell identity and carrier frequency of the current PSCell:

6> set field *timeSpent* to the time spent in the current PSCell while being connected to the current PCell;

4> else:

5> for the newest entry of the PCell in the *mobilityHistoryReport*, include a new entry in the *visitedPSCellInfoListReport,* possibly after removing the oldest PSCell entry of a PCell in the *mobilityHistoryReport*, if required, and set its fields as follows:

6> set field *timeSpent* to the time spent without PSCell in the current PCell since connected to the current PCell in RRC\_CONNECTED;

1> if the *successHO-ReportReq* is set to *true* and if the UE has successful handover related information available in *VarSuccessHO-Report* and if the RPLMN is included in the *plmn-IdentityList* stored in *VarSuccessHO-Report*:

2> if the *successHO-Report* in the *VarSuccessHO-Report* concerns a DAPS handover and if a PDCP PDU has been received from the source cell of the concerned HO and a non-duplicated PDCP PDU has been received from the target cell of the concerned HO:

3> set *upInterruptionTimeAtHO* in *VarSuccessHO-Report* to include the time elapsed between the time of arrival of the last PDCP PDU received from the source cell of the concerned handover and the time of arrival of the first non-duplicate PDCP PDU received from the target cell of the concerned handover, as measured at the time of arrival of the first non-duplicate PDCP PDU received from the target cell;

2> set the *successHO-Report* in the *UEInformationResponse* message to the value of *successHO-Report* in the *VarSuccessHO-Report*, if available;

2> discard the *VarSuccessHO-Report* upon successful delivery of the *UEInformationResponse* message confirmed by lower layers;

1> if the *coarseLocationRequest* is set to *true*:

2> include *coarseLocationInfo,* if available;

1> if the *logMeasReport* is included in the *UEInformationResponse*:

2> submit the *UEInformationResponse* message to lower layers for transmission via SRB2;

2> discard the logged measurement entries included in the *logMeasInfoList* from *VarLogMeasReport* upon successful delivery of the *UEInformationResponse* message confirmed by lower layers;

1> else:

2> submit the *UEInformationResponse* message to lower layers for transmission via SRB1.

5.7.10.4 Actions upon successful completion of a random-access procedure or on completion of a request of on-demand system information

Upon successfully performing random-access procedure initialized with 4-step or 2-step RA type, or upon failed or successfully completed on-demand system information acquisition procedure in RRC\_IDLE or RRC\_INACTIVE state, the UE shall:

1> if the RPLMN or the PLMN selected by upper layers (see TS24.501 [23]) from the PLMN(s) included in the *plmn-IdentityList* in *SIB1* is not included in *plmn-IdentityList* stored in a non-empty *VarRA-Report*:

2> clear the information included in *VarRA-Report*;

1> if the number of *RA-Report* entries stored in the *ra-ReportList* in *VarRA-Report* is less than *maxRAReport*:

2> if the number of PLMN entries in *plmn-IdentityList* stored in *VarRA-Report* is less than *maxPLMN*; or

2> if the number of PLMN entries in *plmn-IdentityList* stored in *VarRA-Report* is equal to *maxPLMN* and the list of EPLMNs is subset of or equal to the *plmn-IdentityList* stored in *VarRA-Report*:

3> append the following contents associated to the successfully completed random-access procedure or the failed or successfully completed on-demand system information acquisition procedure as a new entry in the *VarRA-Report*:

4> if the list of EPLMNs has been stored by the UE:

5> set the *plmn-IdentityList* to include the list of EPLMNs stored by the UE (i.e. includes the RPLMN) without exceeding the limit of *maxPLMN*;

4> else:

5> set the *plmn-Identity*, in *plmn-IdentityList*, to the PLMN selected by upper layers (see TS 24.501 [23]) from the PLMN(s) included in the *plmn-IdentityInfoList* in SIB1;

4> set the *cellId* to the global cell identity and the tracking area code, if available, otherwise to the physical cell identity and carrier frequency of the cell in which the corresponding random-access preamble was transmitted;

4> if the UE supports spCell ID indication:

5> if the corresponding random-access procedure was performed on an SCell of MCG:

6> set the *spCellId* to the global cell identity of the PCell;

5> if the corresponding random-access procedure was performed on an SCell of SCG; or

5> if the corresponding random-access procedure was performed on PSCell:

6> set the *spCellId* to the global cell identity of the PSCell, if available, otherwise, set the *spCellId* to the global cell identity of the PCell;

4> set the *raPurpose* to include the purpose of triggering the random-access procedure;

4> set the *ra-InformationCommon* as specified in clause 5.7.10.5.

The UE may discard the random access report information, i.e. release the UE variable *VarRA-Report*, 48 hours after the last successful random access procedure or the failed or successfully completed on-demand system information acquisition procedure related information is added to the *VarRA-Report*.

NOTE 1: The UE does not log the RA information in the RA report if the triggering event of the random access is consistent UL LBT on SpCell as specified in TS 38.321 [6].

5.7.10.5 RA information determination

The UE shall set the content in *ra-InformationCommon* as follows:

1> set the *absoluteFrequencyPointA* to indicate the absolute frequency of the reference resource block associated to the random-access resources used in the random-access procedure;

1> set the *locationAndBandwidth* and *subcarrierSpacing* associated to the UL BWP of the random-access resources used in the random-access procedure;

1> if contention based random-access resources are used in the random-access procedure:

2> set the *msgA\_RO-FrequencyStart* and *msgA-RO-FDM* and *msgA-SubcarrierSpacing* associated to the 2 step random- access resources if used in the random-access procedure;

2> if *msgA-SubcarrierSpacing* associated to the 2 step random-access resources used in the random-access procedure is available:

3> set the *msgA-SubcarrierSpacing* associated to the 2 step random-access resources used in the random-access procedure;

2> else if only 2 step random-access resources are available in the UL BWP used in the random-access procedure:

3> set the *msgA-SCS-From-prach-ConfigurationIndex* to the subcarrier spacing as derived from the *msgA-PRACH-ConfigurationIndex* used in the 2-step random-access procedure;

2> else:

3> set the *msg1-SubcarrierSpacing* associated to the 4 step random-access resources used in the random-access procedure;

2> set the *msg1-FrequencyStart* associated to the 4 step random-access resources if used in the random-access procedure, and if its value is different from the value of *msgA-RO-FrequencyStart* if it is included in the *ra-InformationCommon*;

2> set the *msg1-FDM* associated to the 4 step random-access resources if used in the random-access procedure, and if its value is different from the value of *msgA-RO-FDMCFRA* if it is included in the *ra-InformationCommon;*

2> if *msg1-SubcarrierSpacing* associated to the 4 step random-access resources used in the random-access procedure is available, and if its value is different from the value of *msgA-SubcarrierSpacing* if it is included in the *ra-InformationCommon*:

3> set the *msg1-SubcarrierSpacing* associated to the 4 step random-access resources used in the random-access procedure;

2> else:

3> set the *msg1-SCS-From-prach-ConfigurationIndex* to the subcarrier spacing as derived from the *prach-ConfigurationIndex* used in the 4-step random-access procedure, and if its value is different from the value of *msgA-SCS-From-prach-ConfigurationIndex* if it is included in the *ra-InformationCommon*;

1> if contention free random-access resources are used in the random-access procedure:

2> set the *msg1-FrequencyStartCFRA* and *msg1-FDMCFRA* associated to the 4 step random-access resources if used in the random-access procedure;

2> if *msg1-SubcarrierSpacing* associated to the 4 step random-access resources used in the random-access procedure is available:

3> set the *msg1-SubcarrierSpacingCFRA* associated to the 4 step random-access resources used in the random-access procedure;

2> else:

3> set the *msg1-SCS-From-prach-ConfigurationIndexCFRA* to the subcarrier spacing as derived from the *prach-ConfigurationIndex* used in the 4 step random-access procedure;

2> set the *msgA-RO-FrequencyStartCFRA* and *msgA-RO-FDMCFRA* associated to the 2 step contention free random access resources if used in the random-access procedure;

2> set the *msgA-MCS*, the *nrofPRBs-PerMsgA-PO*, the *msgA-PUSCH-TimeDomainAllocation*, the *frequencyStartMsgA-PUSCH*, the *nrofMsgA-PO-FDM* associated to the 2 step random-access resources if used in the random-access procedure;

2> if *msgA-SubcarrierSpacing* associated to the 2 step random-access resources used in the random-access procedure is available:

3> set the *msgA-SubcarrierSpacing* associated to the 2 step random-access resources used in the random-access procedure;

2> else if only 2 step random-access resources are available in the UL BWP used in the random-access procedure:

3> set the *msgA-SCS-From-prach-ConfigurationIndex* to the subcarrier spacing as derived from the *msgA-PRACH-ConfigurationIndex* used in the 2-step random-access procedure;

2> else:

3> set the *msg1-SubcarrierSpacing* associated to the 4 step random-access resources used in the random-access procedure;

1> if the random access procedure is initialized with *RA\_TYPE* set to *2-stepRA* as described in TS 38.321 [3]:

2> set the *dlPathlossRSRP* to the measeured RSRP of the DL pathloss reference obtained at the time of *RA\_Type* selection stage of the initialization of the RA procedure as captured in TS 38.321 [3];

2> if the configuration for the random access *msgA-TransMax* was configured in *RACH-ConfigDedicated* for this random access procedure, and *ra-Purpose* is set to *reconfigurationWithSync*:

3> set *msgA-TransMax* to the value of *msgA-TransMax* in *RACH-ConfigDedicated*;

2> else if *msgA-TransMax* was configured in *RACH-ConfigCommonTwoStepRA*:

3> set *msgA-TransMax* to the value of *msgA-TransMax* in *RACH-ConfigCommonTwoStepRA*;

2> set the *msgA-PUSCH-PayloadSize* to the size of the overall payload available in the UE buffer at the time of initiating the 2 step RA procedure;

1> if the purpose of the random access procedure is to request on-demand system information (i.e., if the *raPurpose* is set to *requestForOtherSI* or *msg3RequestForOtherSI*):

2> set the *intendedSIBs* to indicate the SIB(s) the UE wanted to receive as a result of the SI request;

2> set the *ssbsForSI-Acquisition* to indicate the SSB(s) used to receive the SI message;

2> if the on-demand system information acquisition was successful:

3> set the *onDemandSISuccess* to *true*;

1> set the parameters associated to individual random-access attempt in the chronological order of attempts in the *perRAInfoList* as follows:

2> if the random-access resource used is associated to a SS/PBCH block, set the associated random-access parameters for the successive random-access attempts associated to the same SS/PBCH block for one or more random-access attempts as follows:

3> set the *ssb-Index* to include the SS/PBCH block index associated to the used random-access resource;

3> set the *numberOfPreamblesSentOnSSB* to indicate the number of successive random-access attempts associated to the SS/PBCH block;

3> for each random-access attempt performed on the random-access resource, include the following parameters in the chronological order of the random-access attempt:

4> if the random-access attempt is performed on the contention based random-access resource and if *raPurpose* is not equal to '*requestForOtherSI*', include *contentionDetected* as follows:

5> if contention resolution was not successful as specified in TS 38.321 [6] for the transmitted preamble:

6> set the *contentionDetected* to *true*;

5> else:

6> set the *contentionDetected* to *false*;

4> if the random access attempt is a 2-step random access attempt:

5> if fallback from 2-step random access to 4-step random access occurred during the random access attempt:

6> set *fallbackToFourStepRA* to *true*;

4> if the random-access attempt is performed on the contention based random-access resource; or

4> if the random-access attempt is performed on the contention free random-access resource and if the random-access procedure was initiated due to the PDCCH ordering:

5> if the random access attempt is a 4-step random access attempt and the SS/PBCH block RSRP of the SS/PBCH block corresponding to the random-access resource used in the random-access attempt is above *rsrp-ThresholdSSB*; or

5> if the random access attempt is a 2-step random access attempt and the SS/PBCH block RSRP of the SS/PBCH block corresponding to the random-access resource used in the random-access attempt is above *msgA-RSRP-ThresholdSSB*:

6> set the *dlRSRPAboveThreshold* to *true*;

5> else:

6> set the *dlRSRPAboveThreshold* to *false*;

2> else if the random-access resource used is associated to a CSI-RS, set the associated random-access parameters for the successive random-access attempts associated to the same CSI-RS for one or more random-access attempts as follows:

3> set the *csi-RS-Index* to include the CSI-RS index associated to the used random-access resource;

3> set the *numberOfPreamblesSentOnCSI-RS* to indicate the number of successive random-access attempts associated to the CSI-RS.

NOTE 1: Void.

5

*Next Modified Subclause*

6.2.2 Message definitions

– *RRCRelease*

The *RRCRelease* message is used to command the release of an RRC connection or the suspension of the RRC connection.

Signalling radio bearer: SRB1

RLC-SAP: AM

Logical channel: DCCH

Direction: Network to UE

***RRCRelease* message**

-- ASN1START

-- TAG-RRCRELEASE-START

RRCRelease ::= SEQUENCE {

 rrc-TransactionIdentifier RRC-TransactionIdentifier,

 criticalExtensions CHOICE {

 rrcRelease RRCRelease-IEs,

 criticalExtensionsFuture SEQUENCE {}

 }

}

RRCRelease-IEs ::= SEQUENCE {

 redirectedCarrierInfo RedirectedCarrierInfo OPTIONAL, -- Need N

 cellReselectionPriorities CellReselectionPriorities OPTIONAL, -- Need R

 suspendConfig SuspendConfig OPTIONAL, -- Need R

 deprioritisationReq SEQUENCE {

 deprioritisationType ENUMERATED {frequency, nr},

 deprioritisationTimer ENUMERATED {min5, min10, min15, min30}

 } OPTIONAL, -- Need N

 lateNonCriticalExtension OCTET STRING OPTIONAL,

 nonCriticalExtension RRCRelease-v1540-IEs OPTIONAL

}

RRCRelease-v1540-IEs ::= SEQUENCE {

 waitTime RejectWaitTime OPTIONAL, -- Need N

 nonCriticalExtension RRCRelease-v1610-IEs OPTIONAL

}

RRCRelease-v1610-IEs ::= SEQUENCE {

 voiceFallbackIndication-r16 ENUMERATED {true} OPTIONAL, -- Need N

 measIdleConfig-r16 SetupRelease {MeasIdleConfigDedicated-r16} OPTIONAL, -- Need M

 nonCriticalExtension RRCRelease-v1650-IEs OPTIONAL

}

RRCRelease-v1650-IEs ::= SEQUENCE {

 mpsPriorityIndication-r16 ENUMERATED {true} OPTIONAL, -- Cond Redirection2

 nonCriticalExtension RRCRelease-v1710-IEs OPTIONAL

}

RRCRelease-v1710-IEs ::= SEQUENCE {

 noLastCellUpdate-r17 ENUMERATED {true} OPTIONAL, -- Need S

 nonCriticalExtension RRCRelease-v18xy-IEs OPTIONAL

}

RRCRelease-v18xy-IEs ::= SEQUENCE {

 measIdleConfig-r18 SetupRelease {MeasIdleConfigDedicated-r18} OPTIONAL, -- Need M

 nonCriticalExtension SEQUENCE {} OPTIONAL

}

RedirectedCarrierInfo ::= CHOICE {

 nr CarrierInfoNR,

 eutra RedirectedCarrierInfo-EUTRA,

 ...

}

RedirectedCarrierInfo-EUTRA ::= SEQUENCE {

 eutraFrequency ARFCN-ValueEUTRA,

 cnType ENUMERATED {epc,fiveGC} OPTIONAL -- Need N

}

CarrierInfoNR ::= SEQUENCE {

 carrierFreq ARFCN-ValueNR,

 ssbSubcarrierSpacing SubcarrierSpacing,

 smtc SSB-MTC OPTIONAL, -- Need S

 ...

}

SuspendConfig ::= SEQUENCE {

 fullI-RNTI I-RNTI-Value,

 shortI-RNTI ShortI-RNTI-Value,

 ran-PagingCycle PagingCycle,

 ran-NotificationAreaInfo RAN-NotificationAreaInfo OPTIONAL, -- Need M

 t380 PeriodicRNAU-TimerValue OPTIONAL, -- Need R

 nextHopChainingCount NextHopChainingCount,

 ...,

 [[

 sl-UEIdentityRemote-r17 RNTI-Value OPTIONAL, -- Cond L2RemoteUE

 sdt-Config-r17 SetupRelease { SDT-Config-r17 } OPTIONAL, -- Need M

 srs-PosRRC-Inactive-r17 SetupRelease { SRS-PosRRC-Inactive-r17 } OPTIONAL, -- Need M

 ran-ExtendedPagingCycle-r17 ExtendedPagingCycle-r17 OPTIONAL -- Cond RANPaging

 ]],

 [[

 ncd-SSB-RedCapInitialBWP-SDT-r17 SetupRelease {NonCellDefiningSSB-r17} OPTIONAL -- Need M

 ]]

}

PeriodicRNAU-TimerValue ::= ENUMERATED { min5, min10, min20, min30, min60, min120, min360, min720}

CellReselectionPriorities ::= SEQUENCE {

 freqPriorityListEUTRA FreqPriorityListEUTRA OPTIONAL, -- Need M

 freqPriorityListNR FreqPriorityListNR OPTIONAL, -- Need M

 t320 ENUMERATED {min5, min10, min20, min30, min60, min120, min180, spare1} OPTIONAL, -- Need R

 ...,

 [[

 freqPriorityListDedicatedSlicing-r17 FreqPriorityListDedicatedSlicing-r17 OPTIONAL -- Need M

 ]]

}

PagingCycle ::= ENUMERATED {rf32, rf64, rf128, rf256}

ExtendedPagingCycle-r17 ::= ENUMERATED {rf256, rf512, rf1024, spare1}

FreqPriorityListEUTRA ::= SEQUENCE (SIZE (1..maxFreq)) OF FreqPriorityEUTRA

FreqPriorityListNR ::= SEQUENCE (SIZE (1..maxFreq)) OF FreqPriorityNR

FreqPriorityEUTRA ::= SEQUENCE {

 carrierFreq ARFCN-ValueEUTRA,

 cellReselectionPriority CellReselectionPriority,

 cellReselectionSubPriority CellReselectionSubPriority OPTIONAL -- Need R

}

FreqPriorityNR ::= SEQUENCE {

 carrierFreq ARFCN-ValueNR,

 cellReselectionPriority CellReselectionPriority,

 cellReselectionSubPriority CellReselectionSubPriority OPTIONAL -- Need R

}

RAN-NotificationAreaInfo ::= CHOICE {

 cellList PLMN-RAN-AreaCellList,

 ran-AreaConfigList PLMN-RAN-AreaConfigList,

 ...

}

PLMN-RAN-AreaCellList ::= SEQUENCE (SIZE (1.. maxPLMNIdentities)) OF PLMN-RAN-AreaCell

PLMN-RAN-AreaCell ::= SEQUENCE {

 plmn-Identity PLMN-Identity OPTIONAL, -- Need S

 ran-AreaCells SEQUENCE (SIZE (1..32)) OF CellIdentity

}

PLMN-RAN-AreaConfigList ::= SEQUENCE (SIZE (1..maxPLMNIdentities)) OF PLMN-RAN-AreaConfig

PLMN-RAN-AreaConfig ::= SEQUENCE {

 plmn-Identity PLMN-Identity OPTIONAL, -- Need S

 ran-Area SEQUENCE (SIZE (1..16)) OF RAN-AreaConfig

}

RAN-AreaConfig ::= SEQUENCE {

 trackingAreaCode TrackingAreaCode,

 ran-AreaCodeList SEQUENCE (SIZE (1..32)) OF RAN-AreaCode OPTIONAL -- Need R

}

SDT-Config-r17 ::= SEQUENCE {

 sdt-DRB-List-r17 SEQUENCE (SIZE (0..maxDRB)) OF DRB-Identity OPTIONAL, -- Need M

 sdt-SRB2-Indication-r17 ENUMERATED {allowed} OPTIONAL, -- Need R

 sdt-MAC-PHY-CG-Config-r17 SetupRelease {SDT-CG-Config-r17} OPTIONAL, -- Need M

 sdt-DRB-ContinueROHC-r17 ENUMERATED { cell, rna } OPTIONAL -- Need S

}

SDT-CG-Config-r17 ::= OCTET STRING (CONTAINING SDT-MAC-PHY-CG-Config-r17)

SDT-MAC-PHY-CG-Config-r17 ::= SEQUENCE {

 -- CG-SDT specific configuration

 cg-SDT-ConfigLCH-RestrictionToAddModList-r17 SEQUENCE (SIZE(1..maxLC-ID)) OF CG-SDT-ConfigLCH-Restriction-r17 OPTIONAL, -- Need N

 cg-SDT-ConfigLCH-RestrictionToReleaseList-r17 SEQUENCE (SIZE(1..maxLC-ID)) OF LogicalChannelIdentity OPTIONAL, -- Need N

 cg-SDT-ConfigInitialBWP-NUL-r17 SetupRelease {BWP-UplinkDedicatedSDT-r17} OPTIONAL, -- Need M

 cg-SDT-ConfigInitialBWP-SUL-r17 SetupRelease {BWP-UplinkDedicatedSDT-r17} OPTIONAL, -- Need M

 cg-SDT-ConfigInitialBWP-DL-r17 BWP-DownlinkDedicatedSDT-r17 OPTIONAL, -- Need M

 cg-SDT-TimeAlignmentTimer-r17 TimeAlignmentTimer OPTIONAL, -- Need M

 cg-SDT-RSRP-ThresholdSSB-r17 RSRP-Range OPTIONAL, -- Need M

 cg-SDT-TA-ValidationConfig-r17 SetupRelease { CG-SDT-TA-ValidationConfig-r17 } OPTIONAL, -- Need M

 cg-SDT-CS-RNTI-r17 RNTI-Value OPTIONAL, -- Need M

 ...

}

CG-SDT-TA-ValidationConfig-r17 ::= SEQUENCE {

 cg-SDT-RSRP-ChangeThreshold-r17 ENUMERATED { dB2, dB4, dB6, dB8, dB10, dB14, dB18, dB22,

 dB26, dB30, dB34, spare5, spare4, spare3, spare2, spare1}

}

BWP-DownlinkDedicatedSDT-r17 ::= SEQUENCE {

 pdcch-Config-r17 SetupRelease { PDCCH-Config } OPTIONAL, -- Need M

 pdsch-Config-r17 SetupRelease { PDSCH-Config } OPTIONAL, -- Need M

 ...

}

BWP-UplinkDedicatedSDT-r17 ::= SEQUENCE {

 pusch-Config-r17 SetupRelease { PUSCH-Config } OPTIONAL, -- Need M

 configuredGrantConfigToAddModList-r17 ConfiguredGrantConfigToAddModList-r16 OPTIONAL, -- Need N

 configuredGrantConfigToReleaseList-r17 ConfiguredGrantConfigToReleaseList-r16 OPTIONAL, -- Need N

 ...

}

CG-SDT-ConfigLCH-Restriction-r17 ::= SEQUENCE {

 logicalChannelIdentity-r17 LogicalChannelIdentity,

 configuredGrantType1Allowed-r17 ENUMERATED {true} OPTIONAL, -- Need R

 allowedCG-List-r17 SEQUENCE (SIZE (0.. maxNrofConfiguredGrantConfigMAC-1-r16)) OF ConfiguredGrantConfigIndexMAC-r16

 OPTIONAL -- Need R

}

SRS-PosRRC-Inactive-r17 ::= OCTET STRING (CONTAINING SRS-PosRRC-InactiveConfig-r17)

SRS-PosRRC-InactiveConfig-r17 ::= SEQUENCE {

 srs-PosConfigNUL-r17 SRS-PosConfig-r17 OPTIONAL, -- Need R

 srs-PosConfigSUL-r17 SRS-PosConfig-r17 OPTIONAL, -- Need R

 bwp-NUL-r17 BWP OPTIONAL, -- Need S

 bwp-SUL-r17 BWP OPTIONAL, -- Need S

 inactivePosSRS-TimeAlignmentTimer-r17 TimeAlignmentTimer OPTIONAL, -- Need M

 inactivePosSRS-RSRP-ChangeThreshold-r17 RSRP-ChangeThreshold-r17 OPTIONAL -- Need M

}

RSRP-ChangeThreshold-r17 ::= ENUMERATED {dB4, dB6, dB8, dB10, dB14, dB18, dB22, dB26, dB30, dB34, spare6, spare5, spare4, spare3, spare2, spare1}

SRS-PosConfig-r17 ::= SEQUENCE {

 srs-PosResourceSetToReleaseList-r17 SEQUENCE (SIZE(1..maxNrofSRS-PosResourceSets-r16)) OF SRS-PosResourceSetId-r16 OPTIONAL,-- Need N

 srs-PosResourceSetToAddModList-r17 SEQUENCE (SIZE(1..maxNrofSRS-PosResourceSets-r16)) OF SRS-PosResourceSet-r16 OPTIONAL,-- Need N

 srs-PosResourceToReleaseList-r17 SEQUENCE (SIZE(1..maxNrofSRS-PosResources-r16)) OF SRS-PosResourceId-r16 OPTIONAL,-- Need N

 srs-PosResourceToAddModList-r17 SEQUENCE (SIZE(1..maxNrofSRS-PosResources-r16)) OF SRS-PosResource-r16 OPTIONAL -- Need N

}

-- TAG-RRCRELEASE-STOP

-- ASN1STOP

|  |
| --- |
| ***RRCRelease-IEs* field descriptions** |
| ***cellReselectionPriorities***Dedicated priorities to be used for cell reselection as specified in TS 38.304 [20]*.* The maximum number of NR carrier frequencies that the network can configure through *FreqPriorityListNR* and *FreqPriorityListDedicatedSlicing* together is eight. If the same frequency is configured in both *FreqPriorityListNR* and *FreqPriorityListDedicatedSlicing*, the frequency is only counted once. |
| ***cnType***Indicate that the UE is redirected to EPC or 5GC. |
| ***deprioritisationReq***Indicates whether the current frequency or RAT is to be de-prioritised. |
| ***deprioritisationTimer***Indicates the period for which either the current carrier frequency or NR is deprioritised. Value *minN* corresponds to N minutes. |
| ***measIdleConfig***Indicates measurement configuration to be stored and used by the UE while in RRC\_IDLE or RRC\_INACTIVE or continued during RRC connection setup/resume. |
| ***mpsPriorityIndication***Indicates the UE can set the establishment cause to mps-PriorityAccess for a new connection following a redirect to NR. If the target RAT is E-UTRA, see TS 36.331 [10]. The gNB sets the indication only for UEs authorized to receive MPS treatment as indicated by ARP and/or QoS characteristics at the gNB, and it is applicable only for this instance of release with redirection to carrier/RAT included in the *redirectedCarrierInfo* field in the *RRCRelease* message. |
| ***noLastCellUpdate***Presence of the field indicates that the last used cell for PEI shall not be updated. When the field is absent, the PEI-capable UE shall update its last used cell with the current cell. The UE shall not update its last used cell with the current cell if the AS security is not activated. |
| ***srs-PosRRC-InactiveConfig***SRS for positioning configuration during RRC\_INACTIVE state. |
| ***suspendConfig***Indicates configuration for the RRC\_INACTIVE state. The network does not configure *suspendConfig* when the network redirect the UE to an inter-RAT carrier frequency or if the UE is configured with a DAPS bearer. |
| ***redirectedCarrierInfo***Indicates a carrier frequency (downlink for FDD) and is used to redirect the UE to an NR or an inter-RAT carrier frequency, by means of cell selection at transition to RRC\_IDLE or RRC\_INACTIVE as specified in TS 38.304 [20]. Based on UE capability, the network may include *redirectedCarrierInfo* in *RRCRelease* message with *suspendConfig* if this message is sent in response to an *RRCResumeRequest* or an *RRCResumeRequest1* which is triggered by the NAS layer (see 5.3.1.4 in TS 24.501 [23]). |
| ***voiceFallbackIndication***Indicates the RRC release is triggered by EPS fallback for IMS voice as specified in TS 23.502 [43]. |

|  |
| --- |
| ***CarrierInfoNR* field descriptions** |
| ***carrierFreq***Indicates the redirected NR frequency. |
| ***ssbSubcarrierSpacing***Subcarrier spacing of SSB in the redirected SSB frequency.Only the following values are applicable depending on the used frequency:FR1: 15 or 30 kHzFR2-1: 120 or 240 kHzFR2-2: 120, 480, or 960 kHz |
| ***smtc***The SSB periodicity/offset/duration configuration for the redirected SSB frequency. It is based on timing reference of PCell. If the field is absent, the UE uses the SMTC configured in the measObjectNR having the same SSB frequency and subcarrier spacing. |

|  |
| --- |
| ***RAN-NotificationAreaInfo* field descriptions** |
| ***cellList***A list of cells configured as RAN area. |
| ***ran-AreaConfigList***A list of RAN area codes or RA code(s) as RAN area. |

|  |
| --- |
| ***PLMN-RAN-AreaConfig* field descriptions** |
| ***plmn-Identity***PLMN Identity to which the cells in *ran-Area* belong. If the field is absent the UE not in SNPN access mode uses the ID of the registered PLMN. This field is not included for UE in SNPN access mode (for UE in SNPN access mode the *ran-Area* always belongs to the registered SNPN). |
| ***ran-AreaCodeList***The total number of RAN-AreaCodes of all PLMNs does not exceed 32. |
| ***ran-Area***Indicates whether TA code(s) or RAN area code(s) are used for the RAN notification area. The network uses only TA code(s) or both TA code(s) and RAN area code(s) to configure a UE. The total number of TACs across all PLMNs does not exceed 16. |

|  |
| --- |
| ***PLMN-RAN-AreaCell* field descriptions** |
| ***plmn-Identity***PLMN Identity to which the cells in *ran-AreaCells* belong. If the field is absent the UE not in SNPN access mode uses the ID of the registered PLMN. This field is not included for UE in SNPN access mode (for UE in SNPN access mode the *ran-AreaCells* always belongs to the registered SNPN). |
| ***ran-AreaCells***The total number of cells of all PLMNs does not exceed 32. |

|  |
| --- |
| ***SDT-Config* field descriptions** |
| ***sdt-DRB-ContinueROHC***Indicates whether the PDCP entity of the radio bearers configured for SDT continues or resets the ROHC header compression protocol during PDCP re-establishment during SDT procedure, as specified in TS 38.323 [5]. Value *cell* indicates that ROHC header compression continues when the UE resumes for SDT in the same cell as the PCell when the RRCRelease message was received. Value *rna* indicates that ROHC header compression continues when the UE resumes for SDT in a cell belonging to the same RNA as the PCell where the RRCRelease message was received. If the field is absent, the UE releases any stored value for this field and the PDCP entity of the radio bearers configured for SDT always resets the ROHC header compression protocol during PDCP re-establishment when SDT procedure is initiated, as specified in TS 38.323 [5]. |
| ***sdt-DRB-List***Indicates the ID(s) of the DRB(s) that are configured for SDT. If size of the sequence is zero, then the UE assumes that none of the DRBs are configured for SDT. The network only configures MN terminated MCG bearers for SDT. |
| ***sdt-SRB2-Indication***Indiates whether SRB2 is configured for SDT or not. |

|  |
| --- |
| ***SDT-MAC-PHY-CG-Config* field descriptions** |
| ***cg-SDT-ConfigInitialBWP-DL***Downlink BWP configuration for CG-SDT. If a UE is a RedCap UE and if the *initialDownlinkBWP-RedCap* is configured in *downlinkConfigCommon* in *SIB1*, this field is configured for *initialDownlinkBWP-RedCap*, otherwise it is configured for *initialDownlinkBWP*. |
| ***cg-SDT-ConfigInitialBWP-NUL***UL BWP configuration for CG-SDT on NUL carrier. If a UE is a RedCap UE and if the *initialUplinkBWP-RedCap* is configured in *uplinkConfigCommon* in *SIB1*, this field is configured for *initialUplinkBWP-RedCap*, otherwise it is configured for *initialUplinkBWP* for NUL. |
| ***cg-SDT-ConfigInitialBWP-SUL***UL BWP configuration for CG-SDT on SUL carrier configured for the *initialUplinkBWP* for SUL. |
| ***cg-SDT-CS-RNTI***The CS-RNTI value for CG-SDT as specified in TS 38.321 [3]. |
| ***cg-SDT-RSRP-ThresholdSSB***An RSRP threshold configured for SSB selection for CG-SDT as specified in TS 38.321 [3]. |
| ***cg-SDT-TA-ValidationConfig***Configuration for the RSRP based TA validation. If this field is not configured, then the UE does not perform RSRP based TA validation. |
| ***cg-SDT-timeAlignmentTimer***TAT value for CG-SDT as specified in TS 38.321 [3]. The network always configures this field when *sdt-MAC-PHY-CG-Config* is configured. |

|  |
| --- |
| ***CG-SDT-ConfigLCH-Restriction* field descriptions** |
| ***allowedCG-List***This restriction applies only when the UL grant is a configured grant for CG-SDT. If present, UL MAC SDUs from this logical channel can only be mapped to the indicated CG-SDT configured grant configuration. If the size of the sequence is zero, then UL MAC SDUs from this logical channel cannot be mapped to any CG-SDT configured grant configurations. If the field is not present, UL MAC SDUs from this logical channel can be mapped to any CG-SDT configured grant configurations. If the field *configuredGrantType1Allowed* is present, only those CG-SDT configured grant type 1 configurations indicated in this sequence are allowed for use by this logical channel; otherwise, this sequence shall not include any CG-SDT configured grant type 1 configuration. Corresponds to "*allowedCG*-*List*" as specified in TS 38.321 [3]. |
| ***configuredGrantType1Allowed***If present, or if the capability *lcp-Restriction* as specified in TS 38.306 [26] is not supported, UL MAC SDUs from this logical channel can be transmitted on a configured grant type 1 for CG-SDT. Otherwise, UL MAC SDUs from this logical channel cannot be transmitted on a configured grant type 1 for CG-SDT. Corresponds to "*configuredGrantType1Allowed*" in TS 38.321 [3]. |
| ***logicalChannelIdentity***ID used commonly for the MAC logical channel and for the RLC bearer associated with a *servedRadioBearer* configured for SDT. |

|  |
| --- |
| ***CG-SDT-TA-ValidationConfig* field descriptions** |
| ***cg-SDT-RSRP-ChangeThreshold***The RSRP threshold for TA validation for CG-SDT as specified in TS 38.321 [3]. Value *dB2* corresponds to 2 dB, value *dB4* corresponds to 4 dB and so on. |

|  |
| --- |
| ***SRS-PosRRC-InactiveConfig* field descriptions** |
| ***bwp-NUL***BWP configuration for SRS for Positioning during the RRC\_INACTIVE state in Normal Uplink Carrier. If the field is absent UE is configured with an SRS for Positioning associated with the initial UL BWP and transmitted, during the RRC\_INACTIVE state, inside the initial UL BWP with the same CP and SCS as configured for initial UL BWP. |
| ***bwp-SUL***BWP configuration for SRS for Positioning during the RRC\_INACTIVE state in Supplementary Uplink Carrier. If the field is absent UE is configured with an SRS for Positioning associated with the initial UL BWP and transmitted, during the RRC\_INACTIVE state, inside the initial UL BWP with the same CP and SCS as configured for initial UL BWP. |
| ***inactivePosSRS-RSRP-ChangeThreshold***RSRP threshold for the increase/decrease of RSRP for time alignment validation as specified in TS 38.321 [3]. |
| ***inactivePosSRS-TimeAlignmentTimer***TAT value for SRS for positioning transmission during RRC\_INACTIVE state as specified in TS 38.321 [3]. The network always configures this field when *srs-PosRRC-Inactive* is configured. |
| ***srs-PosConfigNUL***SRS for Positioning configuration in RRC\_INACTIVE state in Normal Uplink Carrier. |
| ***srs-PosConfigSUL***SRS for Positioning configuration in RRC\_INACTIVE state in Supplementary Uplink Carrier. |

|  |
| --- |
| ***SuspendConfig* field descriptions** |
| ***ncd-SSB-RedCapInitialBWP-SDT***Indicates that the UE uses the RedCap-specific initial DL BWP associated with the NCD-SSB for SDT. The network configures this field if a RedCap UE is configured with SDT in the RedCap-specific initial DL BWP not associated with CD-SSB. If configured, the NCD-SSB indicated by this field can only be used during the SDT procedure for CG-SDT or RA-SDT. |
| ***ran-ExtendedPagingCycle***The extended DRX (eDRX) cycle for RAN-initiated paging to be applied by the UE. Value *rf256* corresponds to 256 radio frames, value *rf512* corresponds to 512 radio frames and so on. Value of the field indicates an eDRX cycle which is shorter or equal to the IDLE mode eDRX cycle configured for the UE. |
| ***ran-NotificationAreaInfo***Network ensures that the UE in RRC\_INACTIVE always has a valid *ran-NotificationAreaInfo*. |
| ***ran-PagingCycle***Refers to the UE specific cycle for RAN-initiated paging. Value *rf32* corresponds to 32 radio frames, value *rf64* corresponds to 64 radio frames and so on. |
| ***sl-UEIdentityRemote***Indicates the C-RNTI to the L2 U2N Remote UE. |
| ***t380***Refers to the timer that triggers the periodic RNAU procedure in UE. Value *min5* corresponds to 5 minutes, value *min10* corresponds to 10 minutes and so on. |

|  |  |
| --- | --- |
| **Conditional Presence** | **Explanation** |
| *L2RemoteUE* | The field is mandatory present for L2 U2N Remote UE's RNAU; otherwise it is absent. |
| *RANPaging* | This field is optionally present, Need R, if the UE is configured with IDLE eDRX, see TS 24.501 [23]; otherwise the field is not present. |
| *Redirection2* | The field is optionally present, Need R, if *redirectedCarrierInfo* is included; otherwise the field is not present. |

*Next Modified IE*

– *RRCResume*

The *RRCResume* message is used to resume the suspended RRC connection.

Signalling radio bearer: SRB1

RLC-SAP: AM

Logical channel: DCCH

Direction: Network to UE

***RRCResume* message**

-- ASN1START

-- TAG-RRCRESUME-START

RRCResume ::= SEQUENCE {

 rrc-TransactionIdentifier RRC-TransactionIdentifier,

 criticalExtensions CHOICE {

 rrcResume RRCResume-IEs,

 criticalExtensionsFuture SEQUENCE {}

 }

}

RRCResume-IEs ::= SEQUENCE {

 radioBearerConfig RadioBearerConfig OPTIONAL, -- Need M

 masterCellGroup OCTET STRING (CONTAINING CellGroupConfig) OPTIONAL, -- Need M

 measConfig MeasConfig OPTIONAL, -- Need M

 fullConfig ENUMERATED {true} OPTIONAL, -- Need N

 lateNonCriticalExtension OCTET STRING OPTIONAL,

 nonCriticalExtension RRCResume-v1560-IEs OPTIONAL

}

RRCResume-v1560-IEs ::= SEQUENCE {

 radioBearerConfig2 OCTET STRING (CONTAINING RadioBearerConfig) OPTIONAL, -- Need M

 sk-Counter SK-Counter OPTIONAL, -- Need N

 nonCriticalExtension RRCResume-v1610-IEs OPTIONAL

}

RRCResume-v1610-IEs ::= SEQUENCE {

 idleModeMeasurementReq-r16 ENUMERATED {true} OPTIONAL, -- Need N

 restoreMCG-SCells-r16 ENUMERATED {true} OPTIONAL, -- Need N

 restoreSCG-r16 ENUMERATED {true} OPTIONAL, -- Need N

 mrdc-SecondaryCellGroup-r16 CHOICE {

 nr-SCG-r16 OCTET STRING (CONTAINING RRCReconfiguration),

 eutra-SCG-r16 OCTET STRING

 } OPTIONAL, -- Cond RestoreSCG

 needForGapsConfigNR-r16 SetupRelease {NeedForGapsConfigNR-r16} OPTIONAL, -- Need M

 nonCriticalExtension RRCResume-v1700-IEs OPTIONAL

}

RRCResume-v1700-IEs ::= SEQUENCE {

 sl-ConfigDedicatedNR-r17 SetupRelease {SL-ConfigDedicatedNR-r16} OPTIONAL, -- Cond L2RemoteUE

 sl-L2RemoteUE-Config-r17 SetupRelease {SL-L2RemoteUE-Config-r17} OPTIONAL, -- Cond L2RemoteUE

 needForGapNCSG-ConfigNR-r17 SetupRelease {NeedForGapNCSG-ConfigNR-r17} OPTIONAL, -- Need M

 needForGapNCSG-ConfigEUTRA-r17 SetupRelease {NeedForGapNCSG-ConfigEUTRA-r17} OPTIONAL, -- Need M

 scg-State-r17 ENUMERATED {deactivated} OPTIONAL, -- Need N

 appLayerMeasConfig-r17 AppLayerMeasConfig-r17 OPTIONAL, -- Need M

 nonCriticalExtension RRCResume-v18xy-IEs OPTIONAL

}

RRCResume-v18xy-IEs ::= SEQUENCE {

 fr2-MeasReportReq-r18 ENUMERATED {true} OPTIONAL, -- Need N

 nonCriticalExtension SEQUENCE {} OPTIONAL

}

-- TAG-RRCRESUME-STOP

-- ASN1STOP

|  |
| --- |
| ***RRCResume-IEs* field descriptions** |
| ***appLayerMeasConfig***This field is used to configure application layer measurements. This field is absent when the UE is configured to operate with shared spectrum channel access. |
| ***idleModeMeasurementReq***This field indicates that the UE shall report the idle/inactive measurements, if available, to the network in the *RRCResumeComplete* message |
| ***masterCellGroup***Configuration of the master cell group. |
| ***mrdc-SecondaryCellGroup***Includes an RRC message for SCG configuration in NR-DC or NE-DC.For NR-DC (*nr-SCG*), *mrdc-SecondaryCellGroup* contains the *RRCReconfiguration* message as generated (entirely) by SN gNB. In this version of the specification, the RRC message can only include fields *secondaryCellGroup* (with at least *reconfigurationWithSync*)*,* *otherConfig* and *measConfig*.For NE-DC (*eutra-SCG*), *mrdc-SecondaryCellGroup* includes the E-UTRA *RRCConnectionReconfiguration* message as specified in TS 36.331 [10]. In this version of the specification, the E-UTRA RRC message only include the field *scg-Configuration* with at least *mobilityControlInfoSCG*. |
| ***needForGapsConfigNR***Configuration for the UE to report measurement gap requirement information of NR target bands in the *RRCReconfigurationComplete* and *RRCResumeComplete* message. |
| ***needForGapNCSG-ConfigEUTRA***Configuration for the UE to report measurement gap and NCSG requirement information of E‑UTRA target bands in the *RRCReconfigurationComplete* and *RRCResumeComplete* message. |
| ***needForGapNCSG-ConfigNR***Configuration for the UE to report measurement gap and NCSG requirement information of NR target bands in the *RRCReconfigurationComplete* and *RRCResumeComplete* message. |
| ***radioBearerConfig***Configuration of Radio Bearers (DRBs, SRBs, multicast MRBs) including SDAP/PDCP. |
| ***radioBearerConfig2***Configuration of Radio Bearers (DRBs, SRBs) including SDAP/PDCP. This field can only be used if the UE supports NR-DC or NE-DC. |
| ***restoreMCG-SCells***Indicates that the UE shall restore the MCG SCells from the UE Inactive AS Context, if stored. |
| ***restoreSCG***Indicates that the UE shall restore the SCG configurations from the UE Inactive AS Context, if stored. |
| ***scg-State***Indicates that the SCG is in deactivated state. |
| ***sk-Counter***A counter used to derive S-KgNB or S-KeNB based on the newly derived KgNB during RRC Resume. The field is only included when there is one or more RB with *keyToUse* set to *secondary* *or mrdc-SecondaryCellGroup* is included. |
| ***sl-ConfigDedicatedNR***This field is used to provide the dedicated configurations for NR sidelink communication/discovery used by L2 U2N Remote UE. |
| ***sl-L2RemoteUE-Config***Contains L2 U2N relay operation related configurations used by L2 U2N Remote UE. The field is absent if *appLayerMeasConfig* or SRB4 is configured/not released. |

|  |  |
| --- | --- |
| **Conditional Presence** | **Explanation** |
| *L2RemoteUE* | The field is mandatory present for L2 U2N Remote UE; otherwise it is absent. |
| *RestoreSCG* | The field is mandatory present if *restoreSCG* is included. It is optionally present, Need M, otherwise. |

– *RRCResumeComplete*

The *RRCResumeComplete* message is used to confirm the successful completion of an RRC connection resumption.

Signalling radio bearer: SRB1

RLC-SAP: AM

Logical channel: DCCH

Direction: UE to Network

***RRCResumeComplete* message**

-- ASN1START

-- TAG-RRCRESUMECOMPLETE-START

RRCResumeComplete ::= SEQUENCE {

 rrc-TransactionIdentifier RRC-TransactionIdentifier,

 criticalExtensions CHOICE {

 rrcResumeComplete RRCResumeComplete-IEs,

 criticalExtensionsFuture SEQUENCE {}

 }

}

RRCResumeComplete-IEs ::= SEQUENCE {

 dedicatedNAS-Message DedicatedNAS-Message OPTIONAL,

 selectedPLMN-Identity INTEGER (1..maxPLMN) OPTIONAL,

 uplinkTxDirectCurrentList UplinkTxDirectCurrentList OPTIONAL,

 lateNonCriticalExtension OCTET STRING OPTIONAL,

 nonCriticalExtension RRCResumeComplete-v1610-IEs OPTIONAL

}

RRCResumeComplete-v1610-IEs ::= SEQUENCE {

 idleMeasAvailable-r16 ENUMERATED {true} OPTIONAL,

 measResultIdleEUTRA-r16 MeasResultIdleEUTRA-r16 OPTIONAL,

 measResultIdleNR-r16 MeasResultIdleNR-r16 OPTIONAL,

 scg-Response-r16 CHOICE {

 nr-SCG-Response OCTET STRING (CONTAINING RRCReconfigurationComplete),

 eutra-SCG-Response OCTET STRING

 } OPTIONAL,

 ue-MeasurementsAvailable-r16 UE-MeasurementsAvailable-r16 OPTIONAL,

 mobilityHistoryAvail-r16 ENUMERATED {true} OPTIONAL,

 mobilityState-r16 ENUMERATED {normal, medium, high, spare} OPTIONAL,

 needForGapsInfoNR-r16 NeedForGapsInfoNR-r16 OPTIONAL,

 nonCriticalExtension RRCResumeComplete-v1640-IEs OPTIONAL

}

RRCResumeComplete-v1640-IEs ::= SEQUENCE {

 uplinkTxDirectCurrentTwoCarrierList-r16 UplinkTxDirectCurrentTwoCarrierList-r16 OPTIONAL,

 nonCriticalExtension RRCResumeComplete-v1700-IEs OPTIONAL

}

RRCResumeComplete-v1700-IEs ::= SEQUENCE {

 needForGapNCSG-InfoNR-r17 NeedForGapNCSG-InfoNR-r17 OPTIONAL,

 needForGapNCSG-InfoEUTRA-r17 NeedForGapNCSG-InfoEUTRA-r17 OPTIONAL,

 nonCriticalExtension RRCResumeComplete-v1720-IEs OPTIONAL

}

RRCResumeComplete-v1720-IEs ::= SEQUENCE {

 uplinkTxDirectCurrentMoreCarrierList-r17 UplinkTxDirectCurrentMoreCarrierList-r17 OPTIONAL,

 nonCriticalExtension SEQUENCE {} OPTIONAL

}

RRCResumeComplete-v18xy-IEs ::= SEQUENCE {

 fr2-MeasAvailable-r18 ENUMERATED {available, ongoing } OPTIONAL,

 measResultIdleFR2-NR-r18 MeasResultIdleNR-r18 OPTIONAL,

 nonCriticalExtension SEQUENCE{} OPTIONAL

}

-- TAG-RRCRESUMECOMPLETE-STOP

-- ASN1STOP

|  |
| --- |
| ***RRCResumeComplete-IEs* field descriptions** |
| ***fr2-MeasAvailable***Indication that the UE has FR2 measurement report available for measurements continued during RRC connection resume. |
| ***idleMeasAvailable***Indication that the UE has idle/inactive measurement report available. |
| ***measResultIdleEUTRA***EUTRA measurement results performed during RRC\_INACTIVE. |
| ***measResultIdleNR***NR measurement results performed during RRC\_INACTIVE or continued during RRC connection resume. |
| ***needForGapsInfoNR***This field is used to indicate the measurement gap requirement information of the UE for NR target bands. |
| ***needForGapNCSG-InfoEUTRA***This field is used to indicate the measurement gap and NCSG requirement information of the UE for E‑UTRA target bands |
| ***needForGapNCSG-InfoNR***This field is used to indicate the measurement gap and NCSG requirement information of the UE for NR target bands |
| ***selectedPLMN-Identity***Index of the PLMN selected by the UE from the *plmn-IdentityInfoList* or *npn-IdentityInfoList* fields included in *SIB1*. |
| ***uplinkTxDirectCurrentList***The Tx Direct Current locations for the configured serving cells and BWPs if requested by the NW (see *reportUplinkTxDirectCurrent* in *CellGroupConfig*). |
| ***uplinkTxDirectCurrentMoreCarrierList***The Tx Direct Current locations for the configured intra-band CA requested by *reportUplinkTxDirectCurrentMoreCarrier-r17*. |
| ***uplinkTxDirectCurrentTwoCarrierList***The Tx Direct Current locations for the configured uplink intra-band CA with two carriers if requested by the NW (see *reportUplinkTxDirectCurrentTwoCarrier-r16* in *CellGroupConfig*). |

*Next Modified IE*

– *RRCSetupComplete*

The *RRCSetupComplete* message is used to confirm the successful completion of an RRC connection establishment.

Signalling radio bearer: SRB1

RLC-SAP: AM

Logical channel: DCCH

Direction: UE to Network

***RRCSetupComplete* message**

-- ASN1START

-- TAG-RRCSETUPCOMPLETE-START

RRCSetupComplete ::= SEQUENCE {

 rrc-TransactionIdentifier RRC-TransactionIdentifier,

 criticalExtensions CHOICE {

 rrcSetupComplete RRCSetupComplete-IEs,

 criticalExtensionsFuture SEQUENCE {}

 }

}

RRCSetupComplete-IEs ::= SEQUENCE {

 selectedPLMN-Identity INTEGER (1..maxPLMN),

 registeredAMF RegisteredAMF OPTIONAL,

 guami-Type ENUMERATED {native, mapped} OPTIONAL,

 s-NSSAI-List SEQUENCE (SIZE (1..maxNrofS-NSSAI)) OF S-NSSAI OPTIONAL,

 dedicatedNAS-Message DedicatedNAS-Message,

 ng-5G-S-TMSI-Value CHOICE {

 ng-5G-S-TMSI NG-5G-S-TMSI,

 ng-5G-S-TMSI-Part2 BIT STRING (SIZE (9))

 } OPTIONAL,

 lateNonCriticalExtension OCTET STRING OPTIONAL,

 nonCriticalExtension RRCSetupComplete-v1610-IEs OPTIONAL

}

RRCSetupComplete-v1610-IEs ::= SEQUENCE {

 iab-NodeIndication-r16 ENUMERATED {true} OPTIONAL,

 idleMeasAvailable-r16 ENUMERATED {true} OPTIONAL,

 ue-MeasurementsAvailable-r16 UE-MeasurementsAvailable-r16 OPTIONAL,

 mobilityHistoryAvail-r16 ENUMERATED {true} OPTIONAL,

 mobilityState-r16 ENUMERATED {normal, medium, high, spare} OPTIONAL,

 nonCriticalExtension RRCSetupComplete-v1690-IEs OPTIONAL

}

RRCSetupComplete-v1690-IEs ::= SEQUENCE {

 ul-RRC-Segmentation-r16 ENUMERATED {true} OPTIONAL,

 nonCriticalExtension RRCSetupComplete-v1700-IEs OPTIONAL

}

RRCSetupComplete-v1700-IEs ::= SEQUENCE {

 onboardingRequest-r17 ENUMERATED {true} OPTIONAL,

 nonCriticalExtension RRCSetupComplete-v18xy-IEs OPTIONAL

}

RRCSetupComplete-v18xy-IEs ::= SEQUENCE {

 fr2-MeasAvailable-r18 ENUMERATED {available, ongoing, notAvailable, spare} OPTIONAL,

 nonCriticalExtension SEQUENCE{} OPTIONAL

}

RegisteredAMF ::= SEQUENCE {

 plmn-Identity PLMN-Identity OPTIONAL,

 amf-Identifier AMF-Identifier

}

-- TAG-RRCSETUPCOMPLETE-STOP

-- ASN1STOP

|  |
| --- |
| ***RRCSetupComplete-IEs* field descriptions** |
| ***guami-Type***This field is used to indicate whether the GUAMI included is native (derived from native 5G-GUTI) or mapped (from EPS, derived from EPS GUTI) as specified in TS 24.501 [23]. |
| ***iab-NodeIndication***This field is used to indicate that the connection is being established by an IAB-node as specified in TS 38.300 [2]. |
| ***idleMeasAvailable***Indication that the UE has idle/inactive measurement report available. |
| ***mobilityState***This field indicates the UE mobility state (as defined in TS 38.304 [20], clause 5.2.4.3) just prior to UE going into RRC\_CONNECTED state. The UE indicates the value of *medium* and *high* when being in Medium-mobility and High-mobility states respectively. Otherwise the UE indicates the value *normal*. |
| ***ng-5G-S-TMSI-Part2***The leftmost 9 bits of 5G-S-TMSI. |
| ***onboardingRequest***This field indicates that the connection is being established for UE onboarding in the selected onboarding SNPN, see TS 23.501 [32]. |
| ***registeredAMF***This field is used to transfer the GUAMI of the AMF where the UE is registered, as provided by upper layers, see TS 23.003 [21]. |
| ***selectedPLMN-Identity***Index of the PLMN or SNPN selected by the UE from the *plmn-IdentityInfoList* or *npn-IdentityInfoList* fields included in SIB1. |
| ***ul-RRC-Segmentation***This field indicates the UE supports uplink RRC segmentation of *UECapabilityInformation.* |

*Next Modified IE*

– *SIB1*

*SIB1* contains information relevant when evaluating if a UE is allowed to access a cell and defines the scheduling of other system information.It also contains radio resource configuration information that is common for all UEs and barring information applied to the unified access control.

Signalling radio bearer: N/A

RLC-SAP: TM

Logical channels: BCCH

Direction: Network to UE

***SIB1* message**

-- ASN1START

-- TAG-SIB1-START

SIB1 ::= SEQUENCE {

 cellSelectionInfo SEQUENCE {

 q-RxLevMin Q-RxLevMin,

 q-RxLevMinOffset INTEGER (1..8) OPTIONAL, -- Need S

 q-RxLevMinSUL Q-RxLevMin OPTIONAL, -- Need R

 q-QualMin Q-QualMin OPTIONAL, -- Need S

 q-QualMinOffset INTEGER (1..8) OPTIONAL -- Need S

 } OPTIONAL, -- Cond Standalone

 cellAccessRelatedInfo CellAccessRelatedInfo,

 connEstFailureControl ConnEstFailureControl OPTIONAL, -- Need R

 si-SchedulingInfo SI-SchedulingInfo OPTIONAL, -- Need R

 servingCellConfigCommon ServingCellConfigCommonSIB OPTIONAL, -- Need R

 ims-EmergencySupport ENUMERATED {true} OPTIONAL, -- Need R

 eCallOverIMS-Support ENUMERATED {true} OPTIONAL, -- Need R

 ue-TimersAndConstants UE-TimersAndConstants OPTIONAL, -- Need R

 uac-BarringInfo SEQUENCE {

 uac-BarringForCommon UAC-BarringPerCatList OPTIONAL, -- Need S

 uac-BarringPerPLMN-List UAC-BarringPerPLMN-List OPTIONAL, -- Need S

 uac-BarringInfoSetList UAC-BarringInfoSetList,

 uac-AccessCategory1-SelectionAssistanceInfo CHOICE {

 plmnCommon UAC-AccessCategory1-SelectionAssistanceInfo,

 individualPLMNList SEQUENCE (SIZE (2..maxPLMN)) OF UAC-AccessCategory1-SelectionAssistanceInfo

 } OPTIONAL -- Need S

 } OPTIONAL, -- Need R

 useFullResumeID ENUMERATED {true} OPTIONAL, -- Need R

 lateNonCriticalExtension OCTET STRING OPTIONAL,

 nonCriticalExtension SIB1-v1610-IEs OPTIONAL

}

SIB1-v1610-IEs ::= SEQUENCE {

 idleModeMeasurementsEUTRA-r16 ENUMERATED{true} OPTIONAL, -- Need R

 idleModeMeasurementsNR-r16 ENUMERATED{true} OPTIONAL, -- Need R

 posSI-SchedulingInfo-r16 PosSI-SchedulingInfo-r16 OPTIONAL, -- Need R

 nonCriticalExtension SIB1-v1630-IEs OPTIONAL

}

SIB1-v1630-IEs ::= SEQUENCE {

 uac-BarringInfo-v1630 SEQUENCE {

 uac-AC1-SelectAssistInfo-r16 SEQUENCE (SIZE (2..maxPLMN)) OF UAC-AC1-SelectAssistInfo-r16

 } OPTIONAL, -- Need R

 nonCriticalExtension SIB1-v1700-IEs OPTIONAL

}

SIB1-v1700-IEs ::= SEQUENCE {

 hsdn-Cell-r17 ENUMERATED {true} OPTIONAL, -- Need R

 uac-BarringInfo-v1700 SEQUENCE {

 uac-BarringInfoSetList-v1700 UAC-BarringInfoSetList-v1700

 } OPTIONAL, -- Cond MINT

 sdt-ConfigCommon-r17 SDT-ConfigCommonSIB-r17 OPTIONAL, -- Need R

 redCap-ConfigCommon-r17 RedCap-ConfigCommonSIB-r17 OPTIONAL, -- Need R

 featurePriorities-r17 SEQUENCE {

 redCapPriority-r17 FeaturePriority-r17 OPTIONAL, -- Need R

 slicingPriority-r17 FeaturePriority-r17 OPTIONAL, -- Need R

 msg3-Repetitions-Priority-r17 FeaturePriority-r17 OPTIONAL, -- Need R

 sdt-Priority-r17 FeaturePriority-r17 OPTIONAL -- Need R

 } OPTIONAL, -- Need R

 si-SchedulingInfo-v1700 SI-SchedulingInfo-v1700 OPTIONAL, -- Need R

 hyperSFN-r17 BIT STRING (SIZE (10)) OPTIONAL, -- Need R

 eDRX-AllowedIdle-r17 ENUMERATED {true} OPTIONAL, -- Need R

 eDRX-AllowedInactive-r17 ENUMERATED {true} OPTIONAL, -- Cond EDRX-RC

 intraFreqReselectionRedCap-r17 ENUMERATED {allowed, notAllowed} OPTIONAL, -- Need S

 cellBarredNTN-r17 ENUMERATED {barred, notBarred} OPTIONAL, -- Need S

 nonCriticalExtension SIB1-v1740-IEs OPTIONAL

}

SIB1-v1740-IEs ::= SEQUENCE {

 si-SchedulingInfo-v1740 SI-SchedulingInfo-v1740 OPTIONAL, -- Need R

 nonCriticalExtension SIB1-v18xy-IEs OPTIONAL

}

SIB1-v18xy-IEs ::= SEQUENCE {

 idleModeFR2-MeasurementsNR-r16 ENUMERATED{true} OPTIONAL, -- Need R

 nonCriticalExtension SEQUENCE {} OPTIONAL

}

UAC-AccessCategory1-SelectionAssistanceInfo ::= ENUMERATED {a, b, c}

UAC-AC1-SelectAssistInfo-r16 ::= ENUMERATED {a, b, c, notConfigured}

SDT-ConfigCommonSIB-r17 ::= SEQUENCE {

 sdt-RSRP-Threshold-r17 RSRP-Range OPTIONAL, -- Need R

 sdt-LogicalChannelSR-DelayTimer-r17 ENUMERATED { sf20, sf40, sf64, sf128, sf512, sf1024, sf2560, spare1} OPTIONAL, -- Need R

 sdt-DataVolumeThreshold-r17 ENUMERATED {byte32, byte100, byte200, byte400, byte600, byte800, byte1000, byte2000, byte4000,

 byte8000, byte9000, byte10000, byte12000, byte24000, byte48000, byte96000},

 t319a-r17 ENUMERATED { ms100, ms200, ms300, ms400, ms600, ms1000, ms2000,

 ms3000, ms4000, spare7, spare6, spare5, spare4, spare3, spare2, spare1}

}

RedCap-ConfigCommonSIB-r17 ::= SEQUENCE {

 halfDuplexRedCapAllowed-r17 ENUMERATED {true} OPTIONAL, -- Need R

 cellBarredRedCap-r17 SEQUENCE {

 cellBarredRedCap1Rx-r17 ENUMERATED {barred, notBarred},

 cellBarredRedCap2Rx-r17 ENUMERATED {barred, notBarred}

 } OPTIONAL, -- Need R

 ...

}

FeaturePriority-r17 ::= INTEGER (0..7)

-- TAG-SIB1-STOP

-- ASN1STOP

|  |
| --- |
| ***SIB1* field descriptions** |
| ***cellBarredNTN***Value *barred* means that the cell is barred for connectivity to NTN, as defined in TS 38.304 [20]. Value *notBarred* means that the cell is allowed for connectivity to NTN. If not present, the UE considers the cell is not allowed for connectivity to NTN, as defined in TS 38.304 [20]. This field is only applicable to NTN-capable UEs. |
| ***cellBarredRedCap1Rx***Value *barred* means that the cell is barred for a RedCap UE with 1 Rx branch, as defined in TS 38.304 [20]. This field is ignored by non-RedCap UEs. |
| ***cellBarredRedCap2Rx***Value *barred* means that the cell is barred for a RedCap UE with 2 Rx branches, as defined in TS 38.304 [20]. This field is ignored by non-RedCap UEs. |
| ***cellSelectionInfo***Parameters for cell selection related to the serving cell. |
| ***eCallOverIMS-Support***Indicates whether the cell supports eCall over IMS services as defined in TS 23.501 [32]. If absent, eCall over IMS is not supported by the network in the cell. |
| ***eDRX-AllowedIdle***The presence of this field indicates that extended DRX for CN paging is allowed in the cell for UEs in RRC\_IDLE or RRC\_INACTIVE. The UE shall stop using extended DRX for CN paging in RRC\_IDLE or RRC\_INACTIVE if *eDRX-AllowedIdle* is not present. |
| ***eDRX-AllowedInactive***The presence of this field indicates that extended DRX for RAN paging is allowed in the cell for UEs in RRC\_INACTIVE. The UE shall stop using extended DRX for RAN paging in RRC\_INACTIVE if *eDRX-AllowedInactive* is not present. |
| ***featurePriorities***Indicates priorities for features, such as RedCap, Slicing, SDT and MSG3-Repetitions for Coverage Enhancements. These priorities are used to determine which *FeatureCombinationPreambles* the UE shall use when a feature maps to more than one *FeatureCombinationPreambles*, as specified in TS 38.321 [3]. A lower value means a higher priority. The network does not signal the same priority for more than one feature. The network signals a priority for all feature that map to at least one *FeatureCombinationPreambles*. |
| ***halfDuplexRedCap-Allowed***The presence of this field indicates that the cell supports half-duplex FDD RedCap UEs. |
| ***hsdn-Cell***This field indicates this is a HSDN cell as specified in TS 38.304 [20]. |
| ***hyperSFN***Indicates hyper SFN which increments by one when the SFN wraps around. This field is excluded when determining changes in system information, i.e. changes of hyper SFN should not result in system information change notifications. |
| ***idleModeMeasurementsEUTRA***This field indicates that a UE that is configured for EUTRA idle/inactive measurements shall perform the measurements while camping in this cell and report availability of these measurements when establishing or resuming a connection in this cell. If absent, a UE is not required to perform EUTRA idle/inactive measurements. |
| ***idleModeMeasurementsNR***This field indicates that a UE that is configured for NR idle/inactive measurements shall perform the measurements while camping in this cell and report availability of these measurements when establishing or resuming a connection in this cell. If absent, a UE is not required to perform NR idle/inactive measurements. |
| ***ims-EmergencySupport***Indicates whether the cell supports IMS emergency bearer services for UEs in limited service mode. If absent, IMS emergency call is not supported by the network in the cell for UEs in limited service mode. |
| ***intraFreqReselectionRedCap***Controls cell selection/reselection to intra-frequency cells for RedCap UEs when this cell is barred, or treated as barred by the RedCap UE, as specified in TS 38.304 [20]. If not present, a RedCap UE treats the cell as barred, i.e.,the UE considers that the cell does not support RedCap. |
| ***q-QualMin***Parameter "Qqualmin" in TS 38.304 [20], applicable for serving cell. If the field is absent, the UE applies the (default) value of negative infinity for Qqualmin.  |
| ***q-QualMinOffset***Parameter "Qqualminoffset" in TS 38.304 [20]. Actual value Qqualminoffset = field value [dB]. If the field is absent, the UE applies the (default) value of 0 dB for Qqualminoffset.Affects the minimum required quality level in the cell. |
| ***q-RxLevMin***Parameter "Qrxlevmin" in TS 38.304 [20], applicable for serving cell. |
| ***q-RxLevMinOffset***Parameter "Qrxlevminoffset" in TS 38.304 [20]. Actual value Qrxlevminoffset = field value \* 2 [dB]. If absent, the UE applies the (default) value of 0 dB for Qrxlevminoffset*.* Affects the minimum required Rx level in the cell. |
| ***q-RxLevMinSUL***Parameter "Qrxlevmin" in TS 38.304 [20], applicable for serving cell. |
| ***sdt-RSRP-Threshold***RSRP threshold used to determine whether SDT procedure can be initiated, as specified in TS 38.321 [3]. |
| ***sdt-DataVolumeThreshold***Data volume threshold used to determine whether SDT can be initiated, as specified in TS 38.321 [3]. Value *byte32* corresponds to 32 bytes, value *byte100* corresponds to 100 bytes, and so on. |
| ***sdt-LogicalChannelSR-DelayTimer***The value of *logicalChannelSR-DelayTimer* applied during SDT for logical channels configured with SDT, as specified in TS 38.321 [3]. Value in number of subframes. Value *sf20* corresponds to 20 subframes, *sf40* corresponds to 40 subframes, and so on. If this field is not configured, then logicalChannelSR-DelayTimer is not applied for SDT logical channels. |
| ***servingCellConfigCommon***Configuration of the serving cell. |
| ***t319a***Initial value of the timer T319a used for detection of SDT failure. Value *ms100* corresponds to 100 milliseconds, value *ms200* corresponds to 200 milliseconds and so on. |
| ***uac-AccessCategory1-SelectionAssistanceInfo***Information used to determine whether Access Category 1 applies to the UE, as defined in TS 22.261 [25]. If *plmnCommon* is chosen, the *UAC-AccessCategory1-SelectionAssistanceInfo* is applicable to all the PLMNs and SNPNs in *plmn-IdentityInfoList* and *npn-IdentityInfoList*. If *individualPLMNList* is chosen, the 1st entry in the list corresponds to the first network within all of the PLMNs and SNPNs across the *plmn-IdentityList* and the *npn-IdentityInfoList*, the 2nd entry in the list corresponds to the second network within all of the PLMNs and SNPNs across the *plmn-IdentityList* and the *npn-IdentityInfoList* and so on. If *uac-AC1-SelectAssistInfo-r16* is present, the UE shall ignore the *uac-AccessCategory1-SelectionAssistanceInfo*. |
| ***uac-AC1-SelectAssistInfo***Information used to determine whether Access Category 1 applies to the UE, as defined in TS 22.261 [25]. The 1st entry in the list corresponds to the first network within all of the PLMNs and SNPNs across the *plmn-IdentityList* and *npn-IdentityInfoList*, the 2nd entry in the list corresponds to the second network within all of the PLMNs and SNPNs across the *plmn-IdentityList* and the *npn-IdentityInfoList* and so on. Value *notConfigured* indicates that Access Category1 is not configured for the corresponding PLMN/SNPN. |
| ***uac-BarringForCommon***Common access control parameters for each access category. Common values are used for all PLMNs/SNPNs, unless overwritten by the PLMN/SNPN specific configuration provided in *uac-BarringPerPLMN-List*. The parameters are specified by providing an index to the set of configurations (*uac-BarringInfoSetList*). UE behaviour upon absence of this field is specified in clause 5.3.14.2. |
| ***ue-TimersAndConstants***Timer and constant values to be used by the UE. The cell operating as PCell always provides this field. |
| ***useFullResumeID***Indicates which resume identifier and Resume request message should be used. UE uses *fullI-RNTI* and *RRCResumeRequest1* if the field is present, or *shortI-RNTI* and *RRCResumeRequest* if the field is absent. |

|  |  |
| --- | --- |
| **Conditional Presence** | **Explanation** |
| *EDRX-RC* | The field is optionally present, Need R, in a cell that enables *eDRX-AllowedIdle*, otherwise it is absent. |
| *MINT* | The field is optionally present, Need R, in a cell that provides a configuration for disaster roaming, otherwise it is absent, Need R. |
| *Standalone* | The field is mandatory present in a cell that supports standalone operation, otherwise it is absent. |

*Next Modified IE*

– *UEInformationRequest*

The *UEInformationRequest* message is used by the network to retrieve information from the UE.

Signalling radio bearer: SRB1

RLC-SAP: AM

Logical channel: DCCH

Direction: Network to UE

***UEInformationRequest message***

-- ASN1START

-- TAG-UEINFORMATIONREQUEST-START

UEInformationRequest-r16 ::= SEQUENCE {

 rrc-TransactionIdentifier RRC-TransactionIdentifier,

 criticalExtensions CHOICE {

 ueInformationRequest-r16 UEInformationRequest-r16-IEs,

 criticalExtensionsFuture SEQUENCE {}

 }

}

UEInformationRequest-r16-IEs ::= SEQUENCE {

 idleModeMeasurementReq-r16 ENUMERATED{true} OPTIONAL, -- Need N

 logMeasReportReq-r16 ENUMERATED {true} OPTIONAL, -- Need N

 connEstFailReportReq-r16 ENUMERATED {true} OPTIONAL, -- Need N

 ra-ReportReq-r16 ENUMERATED {true} OPTIONAL, -- Need N

 rlf-ReportReq-r16 ENUMERATED {true} OPTIONAL, -- Need N

 mobilityHistoryReportReq-r16 ENUMERATED {true} OPTIONAL, -- Need N

 lateNonCriticalExtension OCTET STRING OPTIONAL,

 nonCriticalExtension UEInformationRequest-v1700-IEs OPTIONAL

}

UEInformationRequest-v1700-IEs ::= SEQUENCE {

 successHO-ReportReq-r17 ENUMERATED {true} OPTIONAL, -- Need N

 coarseLocationRequest-r17 ENUMERATED {true} OPTIONAL, -- Need N

 nonCriticalExtension UEInformationRequest-v18xy-IEs OPTIONAL

}

UEInformationRequest-v18xy-IEs ::= SEQUENCE {

 fr2-MeasurementReq-r18 ENUMERATED {true} OPTIONAL, -- Need N

 nonCriticalExtension SEQUENCE {} OPTIONAL

}

-- TAG-UEINFORMATIONREQUEST-STOP

-- ASN1STOP

|  |
| --- |
| ***UEInformationRequest-IEs* field descriptions** |
| ***coarseLocationRequest***This field is used to request UE to report coarse location information. |
| ***connEstFailReportReq***This field is used to indicate whether the UE shall report information about the connection failure. |
| ***fr2-MeasurementReq*** This field indicates that the UE shall report the FR2 measurement information for measurements continued during RRC connection setup/resume, if available, to the network in the *UEInformationResponse* message.  |
| ***idleModeMeasurementReq***This field indicates that the UE shall report the idle/inactive measurement information, if available, to the network in the *UEInformationResponse* message.  |
| ***logMeasReportReq***This field is used to indicate whether the UE shall report information about logged measurements. |
| ***mobilityHistoryReportReq***This field is used to indicate whether the UE shall report information about mobility history information. |
| ***ra-ReportReq***This field is used to indicate whether the UE shall report information about the random access procedure. |
| ***rlf-ReportReq***This field is used to indicate whether the UE shall report information about the radio link failure. |
| ***successHO-ReportReq***This field is used to indicate whether the UE shall report information about the successful handover report. |

– *UEInformationResponse*

The *UEInformationResponse* message is used by the UE to transfer information requested by the network.

Signalling radio bearer: SRB1 or SRB2 (when logged measurement information is included)

RLC-SAP: AM

Logical channel: DCCH

Direction: UE to network

***UEInformationResponse message***

-- ASN1START

-- TAG-UEINFORMATIONRESPONSE-START

UEInformationResponse-r16 ::= SEQUENCE {

 rrc-TransactionIdentifier RRC-TransactionIdentifier,

 criticalExtensions CHOICE {

 ueInformationResponse-r16 UEInformationResponse-r16-IEs,

 criticalExtensionsFuture SEQUENCE {}

 }

}

UEInformationResponse-r16-IEs ::= SEQUENCE {

 measResultIdleEUTRA-r16 MeasResultIdleEUTRA-r16 OPTIONAL,

 measResultIdleNR-r16 MeasResultIdleNR-r16 OPTIONAL,

 logMeasReport-r16 LogMeasReport-r16 OPTIONAL,

 connEstFailReport-r16 ConnEstFailReport-r16 OPTIONAL,

 ra-ReportList-r16 RA-ReportList-r16 OPTIONAL,

 rlf-Report-r16 RLF-Report-r16 OPTIONAL,

 mobilityHistoryReport-r16 MobilityHistoryReport-r16 OPTIONAL,

 lateNonCriticalExtension OCTET STRING OPTIONAL,

 nonCriticalExtension UEInformationResponse-v1700-IEs OPTIONAL

}

UEInformationResponse-v1700-IEs ::= SEQUENCE {

 successHO-Report-r17 SuccessHO-Report-r17 OPTIONAL,

 connEstFailReportList-r17 ConnEstFailReportList-r17 OPTIONAL,

 coarseLocationInfo-r17 OCTET STRING OPTIONAL,

 nonCriticalExtension SEQUENCE {} OPTIONAL

}

UEInformationResponse-v18xy-IEs ::= SEQUENCE {

 measResultIdleNR-r18 MeasResultIdleNR-r18 OPTIONAL,

 nonCriticalExtension SEQUENCE {} OPTIONAL

}

LogMeasReport-r16 ::= SEQUENCE {

 absoluteTimeStamp-r16 AbsoluteTimeInfo-r16,

 traceReference-r16 TraceReference-r16,

 traceRecordingSessionRef-r16 OCTET STRING (SIZE (2)),

 tce-Id-r16 OCTET STRING (SIZE (1)),

 logMeasInfoList-r16 LogMeasInfoList-r16,

 logMeasAvailable-r16 ENUMERATED {true} OPTIONAL,

 logMeasAvailableBT-r16 ENUMERATED {true} OPTIONAL,

 logMeasAvailableWLAN-r16 ENUMERATED {true} OPTIONAL,

 ...

}

LogMeasInfoList-r16 ::= SEQUENCE (SIZE (1..maxLogMeasReport-r16)) OF LogMeasInfo-r16

LogMeasInfo-r16 ::= SEQUENCE {

 locationInfo-r16 LocationInfo-r16 OPTIONAL,

 relativeTimeStamp-r16 INTEGER (0..7200),

 servCellIdentity-r16 CGI-Info-Logging-r16 OPTIONAL,

 measResultServingCell-r16 MeasResultServingCell-r16 OPTIONAL,

 measResultNeighCells-r16 SEQUENCE {

 measResultNeighCellListNR MeasResultListLogging2NR-r16 OPTIONAL,

 measResultNeighCellListEUTRA MeasResultList2EUTRA-r16 OPTIONAL

 },

 anyCellSelectionDetected-r16 ENUMERATED {true} OPTIONAL,

 ...,

 [[

 inDeviceCoexDetected-r17 ENUMERATED {true} OPTIONAL

 ]]

}

ConnEstFailReport-r16 ::= SEQUENCE {

 measResultFailedCell-r16 MeasResultFailedCell-r16,

 locationInfo-r16 LocationInfo-r16 OPTIONAL,

 measResultNeighCells-r16 SEQUENCE {

 measResultNeighCellListNR MeasResultList2NR-r16 OPTIONAL,

 measResultNeighCellListEUTRA MeasResultList2EUTRA-r16 OPTIONAL

 },

 numberOfConnFail-r16 INTEGER (1..8),

 perRAInfoList-r16 PerRAInfoList-r16,

 timeSinceFailure-r16 TimeSinceFailure-r16,

 ...

}

ConnEstFailReportList-r17 ::= SEQUENCE (SIZE (1..maxCEFReport-r17)) OF ConnEstFailReport-r16

MeasResultServingCell-r16 ::= SEQUENCE {

 resultsSSB-Cell MeasQuantityResults,

 resultsSSB SEQUENCE{

 best-ssb-Index SSB-Index,

 best-ssb-Results MeasQuantityResults,

 numberOfGoodSSB INTEGER (1..maxNrofSSBs-r16)

 } OPTIONAL

}

MeasResultFailedCell-r16 ::= SEQUENCE {

 cgi-Info CGI-Info-Logging-r16,

 measResult-r16 SEQUENCE {

 cellResults-r16 SEQUENCE{

 resultsSSB-Cell-r16 MeasQuantityResults

 },

 rsIndexResults-r16 SEQUENCE{

 resultsSSB-Indexes-r16 ResultsPerSSB-IndexList

 }

 }

}

RA-ReportList-r16 ::= SEQUENCE (SIZE (1..maxRAReport-r16)) OF RA-Report-r16

RA-Report-r16 ::= SEQUENCE {

 cellId-r16 CHOICE {

 cellGlobalId-r16 CGI-Info-Logging-r16,

 pci-arfcn-r16 PCI-ARFCN-NR-r16

 },

 ra-InformationCommon-r16 RA-InformationCommon-r16 OPTIONAL,

 raPurpose-r16 ENUMERATED {accessRelated, beamFailureRecovery, reconfigurationWithSync, ulUnSynchronized,

 schedulingRequestFailure, noPUCCHResourceAvailable, requestForOtherSI,

 msg3RequestForOtherSI-r17, spare8, spare7, spare6, spare5, spare4, spare3,

 spare2, spare1},

 ...,

 [[

 spCellID-r17 CGI-Info-Logging-r16 OPTIONAL

 ]]

}

RA-InformationCommon-r16 ::= SEQUENCE {

 absoluteFrequencyPointA-r16 ARFCN-ValueNR,

 locationAndBandwidth-r16 INTEGER (0..37949),

 subcarrierSpacing-r16 SubcarrierSpacing,

 msg1-FrequencyStart-r16 INTEGER (0..maxNrofPhysicalResourceBlocks-1) OPTIONAL,

 msg1-FrequencyStartCFRA-r16 INTEGER (0..maxNrofPhysicalResourceBlocks-1) OPTIONAL,

 msg1-SubcarrierSpacing-r16 SubcarrierSpacing OPTIONAL,

 msg1-SubcarrierSpacingCFRA-r16 SubcarrierSpacing OPTIONAL,

 msg1-FDM-r16 ENUMERATED {one, two, four, eight} OPTIONAL,

 msg1-FDMCFRA-r16 ENUMERATED {one, two, four, eight} OPTIONAL,

 perRAInfoList-r16 PerRAInfoList-r16,

 ...,

 [[

 perRAInfoList-v1660 PerRAInfoList-v1660 OPTIONAL

 ]],

 [[

 msg1-SCS-From-prach-ConfigurationIndex-r16 ENUMERATED {kHz1dot25, kHz5, spare2, spare1} OPTIONAL

 ]],

 [[

 msg1-SCS-From-prach-ConfigurationIndexCFRA-r16 ENUMERATED {kHz1dot25, kHz5, spare2, spare1} OPTIONAL

 ]],

 [[

 msgA-RO-FrequencyStart-r17 INTEGER (0..maxNrofPhysicalResourceBlocks-1) OPTIONAL,

 msgA-RO-FrequencyStartCFRA-r17 INTEGER (0..maxNrofPhysicalResourceBlocks-1) OPTIONAL,

 msgA-SubcarrierSpacing-r17 SubcarrierSpacing OPTIONAL,

 msgA-RO-FDM-r17 ENUMERATED {one, two, four, eight} OPTIONAL,

 msgA-RO-FDMCFRA-r17 ENUMERATED {one, two, four, eight} OPTIONAL,

 msgA-SCS-From-prach-ConfigurationIndex-r17 ENUMERATED {kHz1dot25, kHz5, spare2, spare1} OPTIONAL,

 msgA-TransMax-r17 ENUMERATED {n1, n2, n4, n6, n8, n10, n20, n50, n100, n200} OPTIONAL,

 msgA-MCS-r17 INTEGER (0..15) OPTIONAL,

 nrofPRBs-PerMsgA-PO-r17 INTEGER (1..32) OPTIONAL,

 msgA-PUSCH-TimeDomainAllocation-r17 INTEGER (1..maxNrofUL-Allocations) OPTIONAL,

 frequencyStartMsgA-PUSCH-r17 INTEGER (0..maxNrofPhysicalResourceBlocks-1) OPTIONAL,

 nrofMsgA-PO-FDM-r17 ENUMERATED {one, two, four, eight} OPTIONAL,

 dlPathlossRSRP-r17 RSRP-Range OPTIONAL,

 intendedSIBs-r17 SEQUENCE (SIZE (1..maxSIB)) OF SIB-Type-r17 OPTIONAL,

 ssbsForSI-Acquisition-r17 SEQUENCE (SIZE (1..maxNrofSSBs-r16)) OF SSB-Index OPTIONAL,

 msgA-PUSCH-PayloadSize-r17 BIT STRING (SIZE (5)) OPTIONAL,

 onDemandSISuccess-r17 ENUMERATED {true} OPTIONAL

 ]]

}

PerRAInfoList-r16 ::= SEQUENCE (SIZE (1..200)) OF PerRAInfo-r16

PerRAInfoList-v1660 ::= SEQUENCE (SIZE (1..200)) OF PerRACSI-RSInfo-v1660

PerRAInfo-r16 ::= CHOICE {

 perRASSBInfoList-r16 PerRASSBInfo-r16,

 perRACSI-RSInfoList-r16 PerRACSI-RSInfo-r16

}

PerRASSBInfo-r16 ::= SEQUENCE {

 ssb-Index-r16 SSB-Index,

 numberOfPreamblesSentOnSSB-r16 INTEGER (1..200),

 perRAAttemptInfoList-r16 PerRAAttemptInfoList-r16

}

PerRACSI-RSInfo-r16 ::= SEQUENCE {

 csi-RS-Index-r16 CSI-RS-Index,

 numberOfPreamblesSentOnCSI-RS-r16 INTEGER (1..200)

}

PerRACSI-RSInfo-v1660 ::= SEQUENCE {

 csi-RS-Index-v1660 INTEGER (1..96) OPTIONAL

}

PerRAAttemptInfoList-r16 ::= SEQUENCE (SIZE (1..200)) OF PerRAAttemptInfo-r16

PerRAAttemptInfo-r16 ::= SEQUENCE {

 contentionDetected-r16 BOOLEAN OPTIONAL,

 dlRSRPAboveThreshold-r16 BOOLEAN OPTIONAL,

 ...,

 [[

 fallbackToFourStepRA-r17 ENUMERATED {true} OPTIONAL

 ]]

}

SIB-Type-r17 ::= ENUMERATED {sibType2, sibType3, sibType4, sibType5, sibType9, sibType10-v1610, sibType11-v1610, sibType12-v1610,

 sibType13-v1610, sibType14-v1610, spare6, spare5, spare4, spare3, spare2, spare1}

RLF-Report-r16 ::= CHOICE {

 nr-RLF-Report-r16 SEQUENCE {

 measResultLastServCell-r16 MeasResultRLFNR-r16,

 measResultNeighCells-r16 SEQUENCE {

 measResultListNR-r16 MeasResultList2NR-r16 OPTIONAL,

 measResultListEUTRA-r16 MeasResultList2EUTRA-r16 OPTIONAL

 } OPTIONAL,

 c-RNTI-r16 RNTI-Value,

 previousPCellId-r16 CHOICE {

 nrPreviousCell-r16 CGI-Info-Logging-r16,

 eutraPreviousCell-r16 CGI-InfoEUTRALogging

 } OPTIONAL,

 failedPCellId-r16 CHOICE {

 nrFailedPCellId-r16 CHOICE {

 cellGlobalId-r16 CGI-Info-Logging-r16,

 pci-arfcn-r16 PCI-ARFCN-NR-r16

 },

 eutraFailedPCellId-r16 CHOICE {

 cellGlobalId-r16 CGI-InfoEUTRALogging,

 pci-arfcn-r16 PCI-ARFCN-EUTRA-r16

 }

 },

 reconnectCellId-r16 CHOICE {

 nrReconnectCellId-r16 CGI-Info-Logging-r16,

 eutraReconnectCellId-r16 CGI-InfoEUTRALogging

 } OPTIONAL,

 timeUntilReconnection-r16 TimeUntilReconnection-r16 OPTIONAL,

 reestablishmentCellId-r16 CGI-Info-Logging-r16 OPTIONAL,

 timeConnFailure-r16 INTEGER (0..1023) OPTIONAL,

 timeSinceFailure-r16 TimeSinceFailure-r16,

 connectionFailureType-r16 ENUMERATED {rlf, hof},

 rlf-Cause-r16 ENUMERATED {t310-Expiry, randomAccessProblem, rlc-MaxNumRetx,

 beamFailureRecoveryFailure, lbtFailure-r16,

 bh-rlfRecoveryFailure, t312-expiry-r17, spare1},

 locationInfo-r16 LocationInfo-r16 OPTIONAL,

 noSuitableCellFound-r16 ENUMERATED {true} OPTIONAL,

 ra-InformationCommon-r16 RA-InformationCommon-r16 OPTIONAL,

 ...,

 [[

 csi-rsRLMConfigBitmap-v1650 BIT STRING (SIZE (96)) OPTIONAL

 ]],

 [[

 lastHO-Type-r17 ENUMERATED {cho, daps, spare2, spare1} OPTIONAL,

 timeConnSourceDAPS-Failure-r17 TimeConnSourceDAPS-Failure-r17 OPTIONAL,

 timeSinceCHO-Reconfig-r17 TimeSinceCHO-Reconfig-r17 OPTIONAL,

 choCellId-r17 CHOICE {

 cellGlobalId-r17 CGI-Info-Logging-r16,

 pci-arfcn-r17 PCI-ARFCN-NR-r16

 } OPTIONAL,

 choCandidateCellList-r17 ChoCandidateCellList-r17 OPTIONAL

 ]]

 },

 eutra-RLF-Report-r16 SEQUENCE {

 failedPCellId-EUTRA CGI-InfoEUTRALogging,

 measResult-RLF-Report-EUTRA-r16 OCTET STRING,

 ...,

 [[

 measResult-RLF-Report-EUTRA-v1690 OCTET STRING OPTIONAL

 ]]

 }

}

SuccessHO-Report-r17 ::= SEQUENCE {

 sourceCellInfo-r17 SEQUENCE {

 sourcePCellId-r17 CGI-Info-Logging-r16,

 sourceCellMeas-r17 MeasResultSuccessHONR-r17 OPTIONAL,

 rlf-InSourceDAPS-r17 ENUMERATED {true} OPTIONAL

 },

 targetCellInfo-r17 SEQUENCE {

 targetPCellId-r17 CGI-Info-Logging-r16,

 targetCellMeas-r17 MeasResultSuccessHONR-r17 OPTIONAL

 },

 measResultNeighCells-r17 SEQUENCE {

 measResultListNR-r17 MeasResultList2NR-r16 OPTIONAL,

 measResultListEUTRA-r17 MeasResultList2EUTRA-r16 OPTIONAL

 } OPTIONAL,

 locationInfo-r17 LocationInfo-r16 OPTIONAL,

 timeSinceCHO-Reconfig-r17 TimeSinceCHO-Reconfig-r17 OPTIONAL,

 shr-Cause-r17 SHR-Cause-r17 OPTIONAL,

 ra-InformationCommon-r17 RA-InformationCommon-r16 OPTIONAL,

 upInterruptionTimeAtHO-r17 UPInterruptionTimeAtHO-r17 OPTIONAL,

 c-RNTI-r17 RNTI-Value OPTIONAL,

 ...

}

MeasResultList2NR-r16 ::= SEQUENCE(SIZE (1..maxFreq)) OF MeasResult2NR-r16

MeasResultList2EUTRA-r16 ::= SEQUENCE(SIZE (1..maxFreq)) OF MeasResult2EUTRA-r16

MeasResult2NR-r16 ::= SEQUENCE {

 ssbFrequency-r16 ARFCN-ValueNR OPTIONAL,

 refFreqCSI-RS-r16 ARFCN-ValueNR OPTIONAL,

 measResultList-r16 MeasResultListNR

}

MeasResultListLogging2NR-r16 ::= SEQUENCE(SIZE (1..maxFreq)) OF MeasResultLogging2NR-r16

MeasResultLogging2NR-r16 ::= SEQUENCE {

 carrierFreq-r16 ARFCN-ValueNR,

 measResultListLoggingNR-r16 MeasResultListLoggingNR-r16

}

MeasResultListLoggingNR-r16 ::= SEQUENCE (SIZE (1..maxCellReport)) OF MeasResultLoggingNR-r16

MeasResultLoggingNR-r16 ::= SEQUENCE {

 physCellId-r16 PhysCellId,

 resultsSSB-Cell-r16 MeasQuantityResults,

 numberOfGoodSSB-r16 INTEGER (1..maxNrofSSBs-r16) OPTIONAL

}

MeasResult2EUTRA-r16 ::= SEQUENCE {

 carrierFreq-r16 ARFCN-ValueEUTRA,

 measResultList-r16 MeasResultListEUTRA

}

MeasResultRLFNR-r16 ::= SEQUENCE {

 measResult-r16 SEQUENCE {

 cellResults-r16 SEQUENCE{

 resultsSSB-Cell-r16 MeasQuantityResults OPTIONAL,

 resultsCSI-RS-Cell-r16 MeasQuantityResults OPTIONAL

 },

 rsIndexResults-r16 SEQUENCE{

 resultsSSB-Indexes-r16 ResultsPerSSB-IndexList OPTIONAL,

 ssbRLMConfigBitmap-r16 BIT STRING (SIZE (64)) OPTIONAL,

 resultsCSI-RS-Indexes-r16 ResultsPerCSI-RS-IndexList OPTIONAL,

 csi-rsRLMConfigBitmap-r16 BIT STRING (SIZE (96)) OPTIONAL

 } OPTIONAL

 }

}

MeasResultSuccessHONR-r17::= SEQUENCE {

 measResult-r17 SEQUENCE {

 cellResults-r17 SEQUENCE{

 resultsSSB-Cell-r17 MeasQuantityResults OPTIONAL,

 resultsCSI-RS-Cell-r17 MeasQuantityResults OPTIONAL

 },

 rsIndexResults-r17 SEQUENCE{

 resultsSSB-Indexes-r17 ResultsPerSSB-IndexList OPTIONAL,

 resultsCSI-RS-Indexes-r17 ResultsPerCSI-RS-IndexList OPTIONAL

 }

 }

}

ChoCandidateCellList-r17 ::= SEQUENCE(SIZE (1..maxNrofCondCells-r16)) OF ChoCandidateCell-r17

ChoCandidateCell-r17 ::= CHOICE {

 cellGlobalId-r17 CGI-Info-Logging-r16,

 pci-arfcn-r17 PCI-ARFCN-NR-r16

}

SHR-Cause-r17 ::= SEQUENCE {

 t304-cause-r17 ENUMERATED {true} OPTIONAL,

 t310-cause-r17 ENUMERATED {true} OPTIONAL,

 t312-cause-r17 ENUMERATED {true} OPTIONAL,

 sourceDAPS-Failure-r17 ENUMERATED {true} OPTIONAL,

 ...

}

TimeSinceFailure-r16 ::= INTEGER (0..172800)

MobilityHistoryReport-r16 ::= VisitedCellInfoList-r16

TimeUntilReconnection-r16 ::= INTEGER (0..172800)

TimeSinceCHO-Reconfig-r17 ::= INTEGER (0..1023)

TimeConnSourceDAPS-Failure-r17 ::= INTEGER (0..1023)

UPInterruptionTimeAtHO-r17 ::= INTEGER (0..1023)

-- TAG-UEINFORMATIONRESPONSE-STOP

-- ASN1STOP

|  |
| --- |
| ***UEInformationResponse-IEs* field descriptions** |
| ***coarseLocationInfo***Parameter type Ellipsoid-Point defined in TS 37.355 [49]. The first/leftmost bit of the first octet contains the most significant bit. The least significant bits of *degreesLatitude* and *degreesLongitude* are set to 0 to meet the accuracy requirement corresponds to a granularity of approximately 2 km.It is up to UE implementation how many LSBs are set to 0 to meet the accuracy requirement. |
| ***connEstFailReport***This field is used to provide connection establishment failure or connection resume failure information*.* |
| ***connEstFailReportList***This field is used to provide the list of *connEstFailReport* that are stored by the UE for the past up to *maxCEFReport-r17.* |
| ***logMeasReport***This field is used to provide the measurement results stored by the UE associated to logged MDT.  |
| ***measResultIdleEUTRA***EUTRA measurement results performed during RRC\_INACTIVE or RRC\_IDLE. |
| ***measResultIdleNR***NR measurement results performed during RRC\_INACTIVE or RRC\_IDLE, or continued during RRC connection setup/resume. |
| ***ra-ReportList***This field is used to provide the list of RA reports that is stored by the UE for the past upto *maxRAReport-r16* number of successful random access procedures, or failed or successful completion of on-demand system information request procedure. |
| ***rlf-Report***This field is used to indicate the RLF report related contents. |
| ***successHO-Report***This field is used to provide the successful handover report if triggered based on the successful handover configuration. |

|  |
| --- |
| ***LogMeasReport* field descriptions** |
| ***absoluteTimeStamp***Indicates the absolute time when the logged measurement configuration logging is provided, as indicated by NR within *absoluteTimeInfo*. |
| ***anyCellSelectionDetected***This field is used to indicate the detection of *any cell selection* state, as defined in TS 38.304 [20]. The UE sets this field when performing the logging of measurement results in RRC\_IDLE or RRC\_INACTIVE and there is no suitable cell or no acceptable cell. |
| ***inDeviceCoexDetected***Indicates that measurement logging is suspended due to IDC problem detection. |
| ***measResultServingCell***This field refers to the log measurement results taken in the Serving cell. |
| ***numberOfGoodSSB***Indicates the number of good beams (beams that are above *absThreshSS-BlocksConsolidation,* if configured by the network) associated to the cells within the R value range (which is configured by network for cell reselection) of the highest ranked cell as part of the beam level measurements. If the UE has no SSB of a neighbour cell whose measurement quantity is above the *absThreshSS-BlocksConsolidation* or if the network has not configured the *absThreshSS-BlocksConsolidation*, then the UE does not include *numberOfGoodSSB* for the corresponding neighbour cell. If the UE has no SSB of the serving cell whose measurement quantity is above the *absThreshSS-BlocksConsolidation* or if the network has not configured the *absThreshSS-BlocksConsolidation*, then the UE shall set the *numberOfGoodSSB* for the serving cell to one. |
| ***relativeTimeStamp***Indicates the time of logging measurement results, measured relative to the *absoluteTimeStamp*. Value in seconds. |
| ***tce-Id***Parameter Trace Collection Entity Id: See TS 32.422 [52]. |
| ***traceRecordingSessionRef***Parameter Trace Recording Session Reference: See TS 32.422 [52]. |

|  |
| --- |
| ***ConnEstFailReport* field descriptions** |
| ***measResultFailedCell***This field refers to the last measurement results taken in the cell, where connection establishment failure or connection resume failure happened. |
| ***measResultNeighCells***This field refers to the neighbour cell measurements when connection establishment failure or connection resume failure happened. |
| ***numberOfConnFail***This field is used to indicate the latest number of consecutive failed RRCSetup or RRCResume procedures in the same cell independent of RRC state transition. |
| ***timeSinceFailure***This field is used to indicate the time that elapsed since the connection (establishment or resume) failure. Value in seconds. The maximum value 172800 means 172800s or longer. |

|  |
| --- |
| ***RA-InformationCommon* field descriptions** |
| ***absoluteFrequencyPointA***This field indicates the absolute frequency position of the reference resource block (Common RB 0). |
| ***locationAndBandwidth***Frequency domain location and bandwidth of the bandwidth part associated to the random-access resources used by the UE. |
| ***perRAInfoList, perRAInfoList-v1660***This field provides detailed information about each of the random access attempts in the chronological order of the random access attempts. If *perRAInfoList-v1660* is present, it shall contain the same number of entries, listed in the same order as in *perRAInfoList-r16*. |
| ***subcarrierSpacing***Subcarrier spacing used in the BWP associated to the random-access resources used by the UE. |

|  |
| --- |
| ***RA-Report* field descriptions** |
| ***cellID***This field indicates the CGI of the cell in which the associated random access procedure was performed. |
| ***contentionDetected***This field is used to indicate that contention was detected for the transmitted preamble in the given random access attempt or not. This field is not included when the UE performs random access attempt is using contention free random-access resources or when the *raPurpose* is set to *requestForOtherSI* or when the RA attempt is a 2-step RA attempt and fallback to 4-step RA did not occur (i.e. *fallbackToFourStepRA* is not included). |
| ***csi-RS-Index, csi-RS-Index-v1660***This field is used to indicate the CSI-RS index corresponding to the random access attempt.If the random access procedure is for beam failure recovery, the field indicates the NZP-CSI-RS-ResourceId. For CSI-RS index larger than maxNrofCSI-RS-ResourcesRRM-1, the index value is the sum of csi-RS-Index (without suffix) and csi-RS-Index-v1660. |
| ***dlPathlossRSRP***Measeured RSRP of the DL pathloss reference obtained at the time of *RA\_Type* selection stage of the RA procedure as captured in TS 38.321 [3]. |
| ***dlRSRPAboveThreshold***In 4 step random access procedure, this field is used to indicate whether the DL beam (SSB) quality associated to the random access attempt was above or below the threshold *rsrp-ThresholdSSB* in *beamFailureRecoveryConfig* in UL BWP configuration of UL BWP selected for random access procedure initiated for beam failure recovery; Otherwise, *rsrp-ThresholdSSB* in *rach-ConfigCommon* in UL BWP configuration of UL BWP selected for random access procedure.In 2 step random access procedure, this field is used to indicate whether the DL beam (SSB) quality associated to the random access attempt was above or below the threshold *msgA-RSRP-ThresholdSSB* in *rach-ConfigCommonTwoStepRA* in UL BWP configuration of UL BWP selected for random access procedure. |
| ***fallbackToFourStepRA***This field indicates if a fallback indication in MsgB is received (according to TS 38.321 [3]) for the 2-step random access attempt. |
| ***intendedSIBs***This field indicates the SIB(s) the UE wanted to receive as a result of the on demand SI request (when the RA procedure is a used as a SI request) initiated by the UE. That is, it indicates the one(s) of the SIB(s) in the SI message(s) requested to be broadcast that the UE was interested in. |
| ***msg1-SCS-From-prach-ConfigurationIndex***This field is set by the UE with the corresponding SCS for CBRA as derived from the *prach-ConfigurationIndex* in *RACH-ConfigGeneric* when the *msg1-SubcarrierSpacing* is absent; otherwise, this field is absent. |
| ***msg1-SCS-From-prach-ConfigurationIndexCFRA***This field is set by the UE with the corresponding SCS for CFRA as derived from the *prach-ConfigurationIndex* in *RACH-ConfigGeneric* when the *msg1-SubcarrierSpacing* is absent; otherwise, this field is absent. |
| ***msgA-PUSCH-PayloadSize***This field indicates the size of the overall payload available in the UE buffer at the time of initiating the 2 step RA procedure. The value refers to the index of TS 38.321 [3], table 6.1.3.1-1, corresponding to the UE buffer size. |
| ***msgA-RO-FDM***This field indicates the number of msgA PRACH transmission occasions Frequency-Division Multiplexed in one time instance for the PRACH resources configured for 2-step CBRA.. |
| ***msgA-RO-FDMCFRA***This field indicates the number of msgA PRACH transmission occasions Frequency-Division Multiplexed in one time instance for the PRACH resources configured for 2-step CFRA. |
| ***msgA-RO-FrequencyStart***This field indicates the lowest resource block of the contention based random-access resources for 2-step CBRA in the random-access procedure. The indication has the form of the offset of the lowest PRACH transmissions occasion with respect to PRB 0 in the frequency domain. |
| ***msgA-RO-FrequencyStartCFRA***This field indicates the lowest resource block of the contention free random-access resources for the 2-step CFRA in the random-access procedure. The indication has the form of the offset of the lowest PRACH transmissions occasion with respect to PRB 0 in the frequency domain. |
| ***msgA-SCS-From-prach-ConfigurationIndex***This field is set by the UE with the corresponding SCS as derived from the *msgA-PRACH-ConfigurationIndex* in *RACH-ConfigGenericTwoStepRA* (see tables Table 6.3.3.1-1, Table 6.3.3.1-2, Table 6.3.3.2-2 and Table 6.3.3.2-3, TS 38.211 [16]) when the *msgA-SubcarrierSpacing* is absent and when only 2-step random-access resources are available in the UL BWP used in the random-access procedure; otherwise, this field is absent. |
| ***numberOfPreamblesSentOnCSI-RS***This field is used to indicate the total number of successive RA preambles that were transmitted on the corresponding CSI-RS. |
| ***numberOfPreamblesSentOnSSB***This field is used to indicate the total number of successive RA preambles that were transmitted on the corresponding SS/PBCH block. |
| ***onDemandSISuccess***This field is set to *true* when the RA report entry is included because of either msg1 based on demand SI request or msg3 based on demand SI request and if the on-demand SI request is successful. Otherwise, the field is absent. |
| ***perRAAttemptInfoList***This field provides detailed information about a random access attempt. |
| ***perRACSI-RSInfoList***This field provides detailed information about the successive random access attempts associated to the same CSI-RS. |
| ***perRASSBInfoList***This field provides detailed information about the successive random access attempts associated to the same SS/PBCH block. |
| ***ra-InformationCommon***This field is used to provide information on random access attempts. This field is mandatory present. |
| ***raPurpose***This field is used to indicate the RA scenario for which the RA report entry is triggered. The RA accesses associated to Initial access from RRC\_IDLE, RRC re-establishment procedure, transition from RRC-INACTIVE. The indicator *beamFailureRecovery* is used in case of successful beam failure recovery related RA procedure in the SpCell [3]. The indicator *reconfigurationWithSync* is used if the UE executes a reconfiguration with sync. The indicator *ulUnSynchronized* is used if the random access procedure is initiated in a SpCell by DL or UL data arrival during RRC\_CONNECTED when the timeAlignmentTimer is not running in the PTAG or if the RA procedure is initiated in a serving cell by a PDCCH order [3]. The indicator *schedulingRequestFailure* is used in case of SR failures [3]. The indicator *noPUCCHResourceAvailable* is used when the UE has no valid SR PUCCH resources configured [3]. The indicator *requestForOtherSI* is used for MSG1 based on demand SI request. The indicator *msg3RequestForOtherSI* is used in case of MSG3 based SI request. The field can also be used for the SCG-related RA-Report when the *raPurpose* is set to *beamFailureRecovery*, *reconfigurationWithSync*, *ulUnSynchronized*, *schedulingRequestFailure* and *noPUCCHResourceAvailable*. |
| ***spCellID***This field is used to indicate the CGI of the SpCell of the cell group associated to the SCell in which the associated random access procedure was performed. If the UE performs RA procedure on a SCell associated to the MCG, then this field is set to the CGI of the PCell and if the UE performs RA procedure on a SCell associated to the SCG, then this field is set to the CGI of the PSCell. If the CGI of the PSCell is not available at the UE for the RA procedure performed on a SCell associated to the SCG or for the RA procedure on the PSCell, this field is set to the CGI of the PCell. Otherwise, the field is absent. |
| ***ssb-Index***This field is used to indicate the SS/PBCH index of the SS/PBCH block corresponding to the random access attempt. |
| ***ssbsForSI-Acquisition***This field indicates the SSB(s) (in the form of SSB index(es)) that the UE used to receive the requested SI message(s). The field is present if the purpose of the random access procedure was to request on-demand SI (i.e. if the *raPurpose* is set to *requestForOtherSI* or *msg3RequestForOtherSI*). Otherwise, the field is absent. |

|  |
| --- |
| ***RLF-Report* field descriptions** |
| ***choCandidateCellList***This field is used to indicate the list of candidate target cells for conditional handover included in *condRRCReconfig* at the time of connection failure. The field does not include the candidate target cells included in *measResulNeighCells*. |
| ***choCellId***This field is used to indicate the candidate target cell for conditional handover included in *condRRCReconfig* that the UE selected for CHO based recovery while T311 is running. |
| ***connectionFailureType***This field is used to indicate whether the connection failure is due to radio link failure or handover failure. |
| ***csi-rsRLMConfigBitmap,csi-rsRLMConfigBitmap-v1650***These fields are used to indicate the CSI-RS indexes configured in the RLM configurations for the active BWP when the UE declares RLF or HOF. The UE first fills in the *csi-rsRLMConfigBitmap-r16* to indicate the first 96 CSI-RS indexes and then *csi-rsRLMConfigBitmap-v1650* to indicate the latter 96 CSI-RS indexes. The first/leftmost bit in *csi-rsRLMConfigBitmap-r16* corresponds to CSI-RS index 0, the second bit corresponds to CSI-RS index 1. The first/leftmost bit in *csi-rsRLMConfigBitmap-v1650* corresponds to CSI-RS index 96, the second bit corresponds to CSI-RS index 97. These fields are included only if the *RadioLinkMonitoringConfig* for the respective BWP is configured. |
| ***c-RNTI***This field indicates the C-RNTI used in the PCell upon detecting radio link failure or the C-RNTI used in the source PCell upon handover failure. |
| ***failedPCellId***This field is used to indicate the PCell in which RLF is detected or the target PCell of the failed handover. For intra-NR handover *nrFailedPCellId* is included and for the handover from NR to EUTRA *eutraFailedPCellId* is included. The UE sets the ARFCN according to the frequency band used for transmission/ reception when the failure occurred. |
| ***failedPCellId-EUTRA***This field is used to indicate the PCell in which RLF is detected or the source PCell of the failed handover in an E-UTRA RLF report. |
| ***lastHO-Type***This field is used to indicate the type of the last executed handover before the last detected connection failure. The field is set to *cho* if the last executed handover was initiated by a conditional reconfiguration execution. The field is set to *daps* if the last executed handover was a DAPS handover. |
| ***measResultListEUTRA***This field refers to the last measurement results taken in the neighboring EUTRA Cells, when the radio link failure or handover failure happened. |
| ***measResultListNR***This field refers to the last measurement results taken in the neighboring NR Cells, when the radio link failure or handover failure happened. |
| ***measResultLastServCell***This field refers to the log measurement results taken in the PCell upon detecting radio link failure or the source PCell upon handover failure. |
| ***measResult-RLF-Report-EUTRA***Includes the E-UTRA *RLF-Report-r9* IE as specified in TS 36.331 [10]. |
| ***measResult-RLF-Report-EUTRA-v1690***Includes the E-UTRA *RLF-Report-v9e0* IE as specified in TS 36.331 [10]. |
| ***noSuitableCellFound***This field is set by the UE when the T311 expires. |
| ***previousPCellId***This field is used to indicate the source PCell of the last handover (source PCell when the last executed *RRCReconfiguration* message including *reconfigurationWithSync* was received). For intra-NR handover *nrPreviousCell* is included and for the handover from EUTRA to NR *eutraPreviousCell* is included. |
| ***ra-InformationCommon***This field is optionally included when c*onnectionFailureType* is set to 'hof' or when *connectionFailureType* is set to 'rlf' and the *rlf-Cause* equals to 'randomAccessProblem' or 'beamRecoveryFailure'; otherwise this field is absent. |
| ***reconnectCellId***This field is used to indicate the cell in which the UE comes back to connected after connection failure and after failing to perform reestablishment. If the UE comes back to RRC CONNECTED in an NR cell then *nrReconnectCellID* is included and if the UE comes back to RRC CONNECTED in an LTE cell then *eutraReconnectCellID* is included |
| ***reestablishmentCellId***If the UE was not configured with *conditionalReconfiguration* at the time of re-establishment attempt, or if the cell selected for the re-establishment attempt is not a candidate target cell for conditional reconfiguration, this field is used to indicate the cell in which the re-establishment attempt was made after connection failure. |
| ***rlf-Cause***This field is used to indicate the cause of the last radio link failure that was detected. In case of handover failure information reporting (i.e., the *connectionFailureType* is set to '*hof*'), the UE is allowed to set this field to any value, except for the case in which a radio link failure was detected in the source PCell while performing a DAPS handover.. |
| ***ssbRLMConfigBitmap***This field is used to indicate the SS/PBCH block indexes configured in the RLM configurations for the active BWP when the UE declares RLF or HOF.The first/leftmost bit corresponds to SSB index 0, the second bit corresponds to SSB index 1. This field is included only if the *RadioLinkMonitoringConfig* for the respective BWP is configured. |
| ***timeConnFailure***This field is used to indicate the time elapsed since the last HO execution until connection failure. Actual value = field value \* 100ms. The maximum value 1023 means 102.3s or longer. |
| ***timeConnSourceDAPS-Failure***This field is used to indicate the time that elapsed between the last DAPS handover execution and the radio link failure detected in the source cell while T304 is running. Value in milliseconds. The maximum value 1023 means 1023ms or longer. |
| ***timeSinceFailure***This field is used to indicate the time that elapsed since the connection (radio link or handover) failure. Value in seconds. The maximum value 172800 means 172800s or longer. In the case of failure(s) (either at source or at target or at both) associated to DAPS handover, this field indicates the time elapsed since the latest connection (radio link or handover) failure. |
| ***timeSinceCHO-Reconfig***In case of handover failure, this field is used to indicate the time elapsed between the initiation of the last conditional reconfiguration execution towards the target cell and the reception of the latest conditional reconfiguration. In case of radio link failure, this field is used to indicate the time elapsed between the radio link failure and the reception of the latest conditional reconfiguration while connected to the source PCell. Actual value = field value \* 100ms. The maximum value 1023 means 102.3s or longer. |
| ***timeUntilReconnection***This field is used to indicate the time that elapsed between the connection (radio link or handover) failure and the next time the UE comes to RRC CONNECTED in an NR or EUTRA cell, after failing to perform reestablishment. Value in seconds. The maximum value 172800 means 172800s or longer. |

|  |
| --- |
| ***SuccessHO-Report* field descriptions** |
| ***c-RNTI***This field indicates the C-RNTI assigned by the target PCell of the handover for which the successful HO report was generated. |
| ***measResultListNR***This field refers to the last measurement results taken in the neighboring NR Cells when a successful handover is executed. |
| ***rlf-InSourceDAPS***This field indicates whether a radio link failure occurred at the source cell while T304 was running. |
| ***shr-Cause***This field is used to indicate the cause of the successful HO report. |
| ***sourceCellMeas***This field refers to the last measurement results taken in the source PCell of a handover in which the successful handover triggers the *SuccessHO-Report*. |
| ***sourcePCellId***This field is used to indicate the source PCell of a handover in which the successful handover triggers the *SuccessHO-Report*. |
| ***targetCellId***This field is used to indicate the target PCell of a handover in which the successful handover triggers the *SuccessHO-Report*. |
| ***targetCellMeas***This field refers to the last measurement results taken in the target PCell of a handover in which the successful handover triggers the *SuccessHO-Report*. |
| ***timeSinceCHO-Reconfig***This field is used to indicate the time elapsed between the initiation of the last conditional reconfiguration execution towards the target cell and the reception of the latest conditional reconfiguration for this target cell. Actual value = field value \* 100ms. The maximum value 1023 means 102.3s or longer. |
| ***upInterruptionTimeAtHO***This field is used to indicate the time elapsed between the time of arrival of the last PDCP PDU received from the source cell for any data radio bearer and the time of arrival of the first non-duplicate PDCP PDU received from the target cell for any data radio bearer, and it is measured at the time of arrival of the first non-duplicate PDCP PDU received from the target cell for any data radio bearer. The field is set only in case of DAPS handover.Value in milliseconds. The maximum value 1023 means 1023ms or longer. |

*Next Modified Subclause*

6.3.1 System information blocks

*Next Modified IE*

– *SIB11*

*SIB11* contains information related to idle/inactive measurements.

***SIB11* information element**

-- ASN1START

-- TAG-SIB11-START

SIB11-r16 ::= SEQUENCE {

 measIdleConfigSIB-r16 MeasIdleConfigSIB-r16 OPTIONAL, -- Need S

 lateNonCriticalExtension OCTET STRING OPTIONAL,

 ...

}

-- TAG-SIB11-STOP

-- ASN1STOP

| ***SIB11* field descriptions** |
| --- |
| ***measIdleConfigSIB***Indicates measurement configuration to be stored and used by the UE while in RRC\_IDLE or RRC\_INACTIVE. |

*Next Modified Subclause*

6.3.2 Radio resource control information elements

– *MeasIdleConfig*

The IE *MeasIdleConfig* is used to convey information to UE about measurements requested to be done while in RRC\_IDLE or RRC\_INACTIVE or continued during RRC connection setup/resume.

***MeasIdleConfig* information element**

-- ASN1START

-- TAG-MEASIDLECONFIG-START

MeasIdleConfigSIB-r16 ::= SEQUENCE {

 measIdleCarrierListNR-r16 SEQUENCE (SIZE (1..maxFreqIdle-r16)) OF MeasIdleCarrierNR-r16 OPTIONAL, -- Need S

 measIdleCarrierListEUTRA-r16 SEQUENCE (SIZE (1..maxFreqIdle-r16)) OF MeasIdleCarrierEUTRA-r16 OPTIONAL, -- Need S

 ...,

 [[

 measIdleFR2-CarrierNR-r18 MeasIdleCarrierNR-r16 OPTIONAL -- Need S

 ]]

}

MeasIdleConfigDedicated-r16 ::= SEQUENCE {

 measIdleCarrierListNR-r16 SEQUENCE (SIZE (1..maxFreqIdle-r16)) OF MeasIdleCarrierNR-r16 OPTIONAL, -- Need N

 measIdleCarrierListEUTRA-r16 SEQUENCE (SIZE (1..maxFreqIdle-r16)) OF MeasIdleCarrierEUTRA-r16 OPTIONAL, -- Need N

 measIdleDuration-r16 ENUMERATED{sec10, sec30, sec60, sec120, sec180, sec240, sec300, spare},

 validityAreaList-r16 ValidityAreaList-r16 OPTIONAL, -- Need N

 ...

}

MeasIdleConfigDedicated-r18 ::= SEQUENCE {

 measIdleFR2-CarrierNR-r18 MeasIdleCarrierNR-r16 OPTIONAL, -- Need N

 ...

}

ValidityAreaList-r16 ::= SEQUENCE (SIZE (1..maxFreqIdle-r16)) OF ValidityArea-r16

ValidityArea-r16 ::= SEQUENCE {

 carrierFreq-r16 ARFCN-ValueNR,

 validityCellList-r16 ValidityCellList OPTIONAL -- Need N

}

ValidityCellList ::= SEQUENCE (SIZE (1.. maxCellMeasIdle-r16)) OF PCI-Range

MeasIdleCarrierNR-r16 ::= SEQUENCE {

 carrierFreq-r16 ARFCN-ValueNR,

 ssbSubcarrierSpacing-r16 SubcarrierSpacing,

 frequencyBandList MultiFrequencyBandListNR OPTIONAL, -- Need R

 measCellListNR-r16 CellListNR-r16 OPTIONAL, -- Need R

 reportQuantities-r16 ENUMERATED {rsrp, rsrq, both},

 qualityThreshold-r16 SEQUENCE {

 idleRSRP-Threshold-NR-r16 RSRP-Range OPTIONAL, -- Need R

 idleRSRQ-Threshold-NR-r16 RSRQ-Range OPTIONAL -- Need R

 } OPTIONAL, -- Need R

 ssb-MeasConfig-r16 SEQUENCE {

 nrofSS-BlocksToAverage-r16 INTEGER (2..maxNrofSS-BlocksToAverage) OPTIONAL, -- Need S

 absThreshSS-BlocksConsolidation-r16 ThresholdNR OPTIONAL, -- Need S

 smtc-r16 SSB-MTC OPTIONAL, -- Need S

 ssb-ToMeasure-r16 SSB-ToMeasure OPTIONAL, -- Need S

 deriveSSB-IndexFromCell-r16 BOOLEAN,

 ss-RSSI-Measurement-r16 SS-RSSI-Measurement OPTIONAL -- Need S

 } OPTIONAL, -- Need S

 beamMeasConfigIdle-r16 BeamMeasConfigIdle-NR-r16 OPTIONAL, -- Need R

 ...

}

MeasIdleCarrierEUTRA-r16 ::= SEQUENCE {

 carrierFreqEUTRA-r16 ARFCN-ValueEUTRA,

 allowedMeasBandwidth-r16 EUTRA-AllowedMeasBandwidth,

 measCellListEUTRA-r16 CellListEUTRA-r16 OPTIONAL, -- Need R

 reportQuantitiesEUTRA-r16 ENUMERATED {rsrp, rsrq, both},

 qualityThresholdEUTRA-r16 SEQUENCE {

 idleRSRP-Threshold-EUTRA-r16 RSRP-RangeEUTRA OPTIONAL, -- Need R

 idleRSRQ-Threshold-EUTRA-r16 RSRQ-RangeEUTRA-r16 OPTIONAL -- Need R

 } OPTIONAL, -- Need S

 ...

}

CellListNR-r16 ::= SEQUENCE (SIZE (1..maxCellMeasIdle-r16)) OF PCI-Range

CellListEUTRA-r16 ::= SEQUENCE (SIZE (1..maxCellMeasIdle-r16)) OF EUTRA-PhysCellIdRange

BeamMeasConfigIdle-NR-r16 ::= SEQUENCE {

 reportQuantityRS-Indexes-r16 ENUMERATED {rsrp, rsrq, both},

 maxNrofRS-IndexesToReport-r16 INTEGER (1.. maxNrofIndexesToReport),

 includeBeamMeasurements-r16 BOOLEAN

}

RSRQ-RangeEUTRA-r16 ::= INTEGER (-30..46)

-- TAG-MEASIDLECONFIG-STOP

-- ASN1STOP

|  |
| --- |
| ***MeasIdleConfig* field descriptions** |
| ***absThreshSS-BlocksConsolidation***Threshold for consolidation of L1 measurements per RS index. |
| ***beamMeasConfigIdle***Indicates the beam level measurement configuration. |
| ***carrierFreq***Indicates the NR carrier frequency to be used for measurements during RRC\_IDLE or RRC\_INACTIVE. |
| ***carrierFreqEUTRA***Indicates the E-UTRA carrier frequency to be used for measurements during RRC\_IDLE or RRC\_INACTIVE. |
| ***deriveSSB-IndexFromCell***This field indicates whether the UE may use the timing of any detected cell on that frequency to derive the SSB index of all neighbour cells on that frequency. If this field is set to true, the UE assumes SFN and frame boundary alignment across cells on the neighbor frequency as specified in TS 38.133 [14]. |
| ***frequencyBandList***Indicates the list of frequency bands for which the NR idle/inactive measurement parameters apply. The UE shall select the first listed band which it supports in the frequencyBandList field to represent the NR neighbour carrier frequency. |
| ***includeBeamMeasurements***Indicates whether or not the UE shall include beam measurements in the NR idle/inactive measurement results. |
| ***maxNrofRS-IndexesToReport***Max number of beam indices to include in the idle/inactive measurement result. |
| ***measCellListEUTRA***Indicates the list of E-UTRA cells which the UE is requested to measure and report for idle/inactive measurements. |
| ***measCellListNR***Indicates the list of NR cells which the UE is requested to measure and report for idle/inactive measurements. |
| ***measIdleCarrierListEUTRA***Indicates the E-UTRA carriers to be measured during RRC\_IDLE or RRC\_INACTIVE. |
| ***measIdleCarrierListNR***Indicates the NR carriers to be measured during RRC\_IDLE or RRC\_INACTIVE. |
| ***measIdleDuration***Indicates the duration for performing idle/inactive measurements while in RRC\_IDLE or RRC\_INACTIVE. Value sec10 correspond to 10 seconds, value sec30 to 30 seconds and so on. |
| ***nrofSS-BlocksToAverage***Number of SS blocks to average for cell measurement derivation. |
| ***qualityThreshold***Indicates the quality thresholds for reporting the measured cells for idle/inactive NR measurements. |
| ***qualityThresholdEUTRA***Indicates the quality thresholds for reporting the measured cells for idle/inactive E-UTRA measurements. |
| ***reportQuantities***Indicates which measurement quantities UE is requested to report in the idle/inactive measurement report.  |
| ***reportQuantitiesEUTRA***Indicates which E-UTRA measurement quantities the UE is requested to report in the idle/inactive measurement report. |
| ***reportQuantityRS-Indexes***Indicates which measurement information per beam index the UE shall include in the NR idle/inactive measurement results. |
| ***smtc***Indicates the measurement timing configuration for inter-frequency measurement. If this field is absent in *VarMeasIdleConfig*, the UE assumes that SSB periodicity is 5 ms in this frequency. |
| ***ssbSubcarrierSpacing***Indicates subcarrier spacing of SSB.Only the following values are applicable depending on the used frequency:FR1: 15 or 30 kHzFR2-1: 120 or 240 kHzFR2-2: 120, 480, or 960 kHz |
| ***ssb-ToMeasure***The set of SS blocks to be measured within the SMTC measurement duration (see TS 38.215 [9]). When the field is absent in *VarMeasIdleConfig*, the UE measures on all SS-blocks. |
| ***ss-RSSI-Measurement***Indicates the SSB-based RSSI measurement configuration. If the field is absent in *VarMeasIdleConfig*, the UE behaviour is defined in TS 38.215 [89], clause 5.1.3. |
| ***validityAreaList***Indicates the list of frequencies and optionally, for each frequency, a list of cells within which the UE is required to perform measurements while in RRC\_IDLE and RRC\_INACTIVE.  |

*Next Modified Subclause*

– *MeasResultIdleNR*

The IE *MeasResultIdleNR* covers the NR measurement results performed in RRC\_IDLE and RRC\_INACTIVE or continued during RRC connection setup/resume.

***MeasResultIdleNR* information element**

-- ASN1START

-- TAG-MEASRESULTIDLENR-START

MeasResultIdleNR-r16 ::= SEQUENCE {

 measResultServingCell-r16 SEQUENCE {

 rsrp-Result-r16 RSRP-Range OPTIONAL,

 rsrq-Result-r16 RSRQ-Range OPTIONAL,

 resultsSSB-Indexes-r16 ResultsPerSSB-IndexList-r16 OPTIONAL

 },

 measResultsPerCarrierListIdleNR-r16 SEQUENCE (SIZE (1.. maxFreqIdle-r16)) OF MeasResultsPerCarrierIdleNR-r16 OPTIONAL,

 ...

}

MeasResultIdleNR-r18 ::= SEQUENCE {

 measResultServingCell-r16 SEQUENCE {

 rsrp-Result-r16 RSRP-Range OPTIONAL,

 rsrq-Result-r16 RSRQ-Range OPTIONAL,

 resultsSSB-Indexes-r16 ResultsPerSSB-IndexList-r16 OPTIONAL

 },

 measResultsFR2-Carrier-r18 MeasResultIdleNR-r16 OPTIONAL,

 ...

}

MeasResultsPerCarrierIdleNR-r16 ::= SEQUENCE {

 carrierFreq-r16 ARFCN-ValueNR,

 measResultsPerCellListIdleNR-r16 SEQUENCE (SIZE (1..maxCellMeasIdle-r16)) OF MeasResultsPerCellIdleNR-r16,

 ...

}

MeasResultsPerCellIdleNR-r16 ::= SEQUENCE {

 physCellId-r16 PhysCellId,

 measIdleResultNR-r16 SEQUENCE {

 rsrp-Result-r16 RSRP-Range OPTIONAL,

 rsrq-Result-r16 RSRQ-Range OPTIONAL,

 resultsSSB-Indexes-r16 ResultsPerSSB-IndexList-r16 OPTIONAL

 },

 ...

}

ResultsPerSSB-IndexList-r16 ::= SEQUENCE (SIZE (1.. maxNrofIndexesToReport)) OF ResultsPerSSB-IndexIdle-r16

ResultsPerSSB-IndexIdle-r16 ::= SEQUENCE {

 ssb-Index-r16 SSB-Index,

 ssb-Results-r16 SEQUENCE {

 ssb-RSRP-Result-r16 RSRP-Range OPTIONAL,

 ssb-RSRQ-Result-r16 RSRQ-Range OPTIONAL

 } OPTIONAL

}

-- TAG-MEASRESULTIDLENR-STOP

-- ASN1STOP

|  |
| --- |
| ***MeasResultIdleNR* field descriptions** |
| ***carrierFreq***Indicates the NR carrier frequency. |
| ***measIdleResultNR***Idle/inactive measurement results for an NR cell (optionally including beam level measurements). |
| ***measResultServingCell***Measured results of the serving cell (i.e., PCell) from idle/inactive measurements. |
| ***measResultsPerCellListIdleNR***List of idle/inactive measured results for the maximum number of reported best cells for a given NR carrier. |
| ***resultsSSB-Indexes***Beam level measurement results (indexes and optionally, beam measurements). |

*Next Modified Subclause*

7.4 UE variables

– *VarMeasIdleConfig*

The UE variable *VarMeasIdleConfig* includes the configuration of the measurements to be performed by the UE while in RRC\_IDLE or RRC\_INACTIVE for NR inter-frequency and inter-RAT (i.e. EUTRA) measurements.

***VarMeasIdleConfig UE* variable**

-- ASN1START

-- TAG-VARMEASIDLECONFIG-START

VarMeasIdleConfig-r16 ::= SEQUENCE {

 measIdleCarrierListNR-r16 SEQUENCE (SIZE (1..maxFreqIdle-r16)) OF MeasIdleCarrierNR-r16 OPTIONAL,

 measIdleCarrierListEUTRA-r16 SEQUENCE (SIZE (1..maxFreqIdle-r16)) OF MeasIdleCarrierEUTRA-r16 OPTIONAL,

 measIdleDuration-r16 ENUMERATED {sec10, sec30, sec60, sec120, sec180, sec240, sec300, spare},

 validityAreaList-r16 ValidityAreaList-r16 OPTIONAL

}

VarMeasIdleConfig-r18 ::= SEQUENCE {

 measIdleFR2-CarrierNR-r18 MeasIdleCarrierNR-r16 OPTIONAL

}

-- TAG-VARMEASIDLECONFIG-STOP

-- ASN1STOP

– *VarMeasIdleReport*

The UE variable *VarMeasIdleReport* includes the logged measurements information.

***VarMeasIdleReport UE* variable**

-- ASN1START

-- TAG-VARMEASIDLEREPORT-START

VarMeasIdleReport-r16 ::= SEQUENCE {

 measReportIdleNR-r16 MeasResultIdleNR-r16 OPTIONAL,

 measReportIdleEUTRA-r16 MeasResultIdleEUTRA-r16 OPTIONAL

}

VarMeasIdleReport-r18 ::= SEQUENCE {

 measReportIdleNR-r18 MeasResultIdleFR2-NR-r18 OPTIONAL

}

-- TAG-VARMEASIDLEREPORT-STOP

-- ASN1STOP

*Next Modified Subclause*

*End of Changes*