**3GPP TSG-RAN WG2 Meeting #124 *R2-231xxx***

**Chicago, US, November 13-17, 2023**

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  |  | **CR** |  | **rev** |  | **Current version:** |  |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **x** | Radio Access Network | **x** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | UE capabilities for Rel-18 XR WI |
|  |  |
| ***Source to WG:*** | Intel Corporation |
| ***Source to TSG:*** | R2 |
|  |  |
| ***Work item code:*** | NR\_XR\_enh-Core |  | ***Date:*** | 2023-11-17 |
|  |  |  |  |  |
| ***Category:*** |  |  | ***Release:*** | Rel-18 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | Introduction of REl-18 XR capabilities on RAN2-led features |
|  |  |
| ***Summary of change:*** | 1. New abbreviations are added: XR, PSI
2. The following new UE capabilities (defined as optional with signaling):
	1. *additionalBSR-Table-r18*
	2. *delayStatusReport-r18*
	3. *disableCG-RetransmissionMonitoring-r18*
	4. *enhancedDRX-r18*
	5. *pdu-SetDiscard-r18*
	6. *psi-BasedDiscard-r18*
	7. *ul-TrafficInfo-r18*
 |
|  |  |
| ***Consequences if not approved:*** | Rel-18 XR feature is not completed |
|  |  |
| ***Clauses affected:*** | 2, 3.3, 4.2.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** | **x** |  |  Other core specifications  | TS/TR 38.331 CR ...  |
| ***affected:*** |  | **x** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **x** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

1. ***Modified section***

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications".

[2] 3GPP TS 38.101-1: "NR; User Equipment (UE) radio transmission and reception Part 1: Range 1 Standalone".

[3] 3GPP TS 38.101-2: "NR; User Equipment (UE) radio transmission and reception Part 2: Range 2 Standalone".

[4] 3GPP TS 38.101-3: "NR; User Equipment (UE) radio transmission and reception Part 3: Range 1 and Range 2 Interworking operation with other radios".

[5] 3GPP TS 38.133: "NR; Requirements for support of radio resource management".

[6] 3GPP TS 38.211: "NR; Physical channels and modulation".

[7] 3GPP TS 37.340: "Evolved Universal Terrestrial Radio Access (E-UTRA) and NR Multi-connectivity".

[8] 3GPP TS 38.321: "NR; Medium Access Control (MAC) protocol specification".

[9] 3GPP TS 38.331: "NR; Radio Resource Control (RRC) protocol specification".

[10] 3GPP TS 38.212: "NR; Multiplexing and channel coding".

[11] 3GPP TS 38.213: "NR; Physical layer procedures for control".

[12] 3GPP TS 38.214: "NR; Physical layer procedures for data".

[13] 3GPP TS 38.215: "NR; Physical layer measurements".

[14] 3GPP TS 36.101: "Evolved Universal Terrestrial Radio Access (E-UTRA) radio transmission and reception".

[15] 3GPP TS 36.306: "Evolved Universal Terrestrial Radio Access (E-UTRA) User Equipment (UE) radio access capabilities".

[16] 3GPP TS 38.323: "NR; Packet Data Convergence Protocol (PDCP) specification".

[17] 3GPP TS 36.331: "Evolved Universal Terrestrial Radio Access (E-UTRA) Radio Resource Control (RRC); Protocol Specification".

[18] 3GPP TS 38.101-4: "NR; User Equipment (UE) radio transmission and reception Part 4: Performance requirements".

[19] 3GPP TS 36.213: "Evolved Universal Terrestrial Radio Access (E-UTRA); Physical layer procedures".

[20] 3GPP TS 25.306: "UE radio access capabilities".

[21] 3GPP TS 38.304: "User Equipment (UE) procedures in Idle mode and RRC Inactive state".

[22] 3GPP TS 37.355: " LTE Positioning Protocol (LPP)".

[23] 3GPP TS 38.340: "NR; Backhaul Adaptation Protocol (BAP) specification".

[24] 3GPP TR 38.822: "NR; User Equipment (UE) feature list".

[25] 3GPP TS 37.324: "E-UTRA and NR; Service Data Adaptation Protocol (SDAP) specification"

[26] 3GPP TS 38.314: "NR; Layer 2 Measurements".

[27] 3GPP TS 36.133: "Evolved Universal Terrestrial Radio Access (E-UTRA); Requirements for support of radio resource management".

[28] 3GPP TS 38.300: "NR; NR and NG-RAN Overall Description; Stage-2".

[29] 3GPP TS 26.247: "Transparent end-to-end Packet-switched Streaming Service (PSS); Progressive Download and Dynamic Adaptive Streaming over HTTP (3GP-DASH)".

[30] 3GPP TS 26.114: "IP Multimedia Subsystem (IMS); Multimedia Telephony; Media handling and interaction".

[31] 3GPP TS 26.118: "Virtual Reality (VR) profiles for streaming applications".

[32] 3GPP TS 37.213: "Physical layer procedures for shared spectrum channel access".

[33] 3GPP TS 38.401: "NG-RAN; Architecture description".

[34] 3GPP TS 38.101-5: "NR; User Equipment (UE) radio transmission and reception; Part 5: Satellite access Radio Frequency (RF) and performance requirements".

[35] 3GPP TS 38.104: "NR; Base Station (BS) radio transmission and reception".

[x] 3GPP TS 38.322: "NR; Radio Link Control (RLC) protocol specification".

1. ***Modified section***

# 3 Definitions, symbols and abbreviations

<<text omitted>>

## 3.3 Abbreviations

For the purposes of the present document, the abbreviations given in TR 21.905 [1] and the following apply. An abbreviation defined in the present document takes precedence over the definition of the same abbreviation, if any, in TR 21.905 [1].

A-CSI Aperiodic-CSI

BAP Backhaul Adaptation Protocol

BC Band Combination

BPS Body Proximity Sensing

BT Bluetooth

CCS Cross Carrier Scheduling

CMR Channel Measurement Resource

CPAC Conditional PSCell Addition/Change

DAPS Dual Active Protocol Stack

DL Downlink

EHC Ethernet Header Compression

FS Feature Set

FSPC Feature Set Per Component-carrier

GSO Geosynchronous Orbit

HSDN High Speed Dedicated Network

IAB-MT Integrated Access Backhaul Mobile Termination

MAC Medium Access Control

MHI Mobility History Information

MBS Multicast/Broadcast Service

MCG Master Cell Group

MN Master Node

MRB MBS Radio Bearer

MR-DC Multi-Radio Dual Connectivity

mTRP Multiple TRP

MUSIM Multi-Universal Subscriber Identity Module

NCJT Non-Coherent Joint Transmission

NCSG Network Controlled Small Gap

NGSO Non-Geosynchronous Orbit

NTN Non-Terrestrial Network

P-CSI Periodic CSI

PDCP Packet Data Convergence Protocol

PSI PDU Set Importance

QoE Quality of Experience

RLC Radio Link Control

RTT Round Trip Time

SCG Secondary Cell Group

SDAP Service Data Adaptation Protocol

SN Secondary Node

sTRP Serving TRP

TRP Transmit/Receive Point

UDC Uplink Data Compression

UL Uplink

WLAN Wireless Local Area Network

XR eXtended Reality

1. ***Modified section***

# 4 UE radio access capability parameters

<<text omitted>>

## 4.2 UE Capability Parameters

<<text omitted>>

### 4.2.2 General parameters

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Definitions for parameters | Per | M | FDD-TDD DIFF | **FR1-FR2**DIFF |
| ***accessStratumRelease***Indicates the access stratum release the UE supports as specified in TS 38.331 [9]. | UE | Yes | No | No |
| ***additionalBSR-Table-r18***Indicates whether the UE supports the BSR enhancements associated with the additional BSR table as specified in TS 38.321 [8] and 38.331 [9]. | UE | No | No | No |
| ***crossCarrierSchedulingConfigurationRelease-r17***Indicates whether the UE supports using *crossCarrierSchedulingConfigRelease* to release the configurations configured by *crossCarrierSchedulingConfig*. | UE | No | No | No |
| ***delayBudgetReporting***Indicates whether the UE supports delay budget reporting as specified in TS 38.331 [9]. | UE | No | No | No |
| ***delayStatusReport-r18***Indicates whether the UE supports the delay status report of the buffered data as specified in TS 38.321 [8], 38.331 [9], 38.323 [16] and 38.322 [x]. | UE | No | No | No |
| ***disableCG-RetransmissionMonitoring-r18***Indicates whether the UE supports to disable monitoring for retransmissions corresponding to a *ConfiguredGrantConfig* as specified in TS 38.321 [8] and 38.331 [9]. | UE | No | No | No |
| ***dl-DedicatedMessageSegmentation-r16***Indicates whether the UE supports reception of segmented DL RRC messages. | UE | No | No | No |
| ***drx-Preference-r16***Indicates whether the UE supports providing its preference of a cell group on DRX parameters for power saving in RRC\_CONNECTED, as specified in TS 38.331 [9]. | UE | No | No | No |
| ***enhancedDRX-r18***Indicates whether the UE supports DRX enhancements including the support of non-integer DRX periodicity and addressing the SFN wrap around as specified in TS 38.331 [9] and 38.321 [8]. | UE | No | No | No |
| ***gNB-SideRTT-BasedPDC-r17***Indicates whether the UE supports gNB-side RTT-based PDC, as specified in TS 38.300 [28]. A UE supporting this feature shall also support *rtt-BasedPDC-CSI-RS-ForTracking-r17* and/or *rtt-BasedPDC-PRS-r17*. | UE | No | No | No |
| ***inactiveState***Indicates whether the UE supports RRC\_INACTIVE as specified in TS 38.331 [9]. | UE | Yes | No | No |
| ***inactiveStateNTN-r17***Indicates whether the UE supports RRC\_INACTIVE in NTN as specified in TS 38.331 [9]. It is mandated if the UE indicates the support of *nonTerrestrialNetwork-r17*. | UE | CY | No | No |
| ***inactiveStatePO-Determination-r17***Indicates whether the UE supports to use the same i\_s to determine PO in RRC\_INACTIVE state as in RRC\_IDLE state. | UE | No | No | No |
| ***inDeviceCoexInd-r16***Indicates whether the UE supports IDC (In-Device Coexistence) assistance information as specified in TS 38.331 [9]. | UE | No | No | No |
| ***maxBW-Preference-r16, maxBW-Preference-r17***Indicates whether the UE supports providing its preference of a cell group on the maximum aggregated bandwidth for power saving in RRC\_CONNECTED, as specified in TS 38.331 [9]. | UE | No | No | Yes(Incl FR2-2 DIFF) |
| ***maxCC-Preference-r16***Indicates whether the UE supports providing its preference of a cell group on the maximum number of secondary component carriers for power saving in RRC\_CONNECTED, as specified in TS 38.331 [9]. | UE | No | No | No |
| ***maxMIMO-LayerPreference-r16, maxMIMO-LayerPreference-r17***Indicates whether the UE supports providing its preference of a cell group on the maximum number of MIMO layers for power saving in RRC\_CONNECTED, as specified in TS 38.331 [9]. | UE | No | No | Yes(Incl FR2-2 DIFF) |
| ***maxMRB-Add-r17***Indicates the additional maximum number of MRBs that the UE supports for MBS multicast reception as specified in TS 38.331 [9].  | UE | No | No | No |
| ***mcgRLF-RecoveryViaSCG-r16***Indicates whether the UE supports recovery from MCG RLF via split SRB1 (if supported) and via SRB3 (if supported) as specified in TS 38.331[9]. | UE | No | No | No |
| ***minSchedulingOffsetPreference-r16***Indicates whether the UE supports providing its preference on the minimum scheduling offset for cross-slot scheduling of the cell group for power saving in RRC\_CONNECTED, as specified in TS 38.331 [9]. | UE | No | No | No |
| ***mpsPriorityIndication-r16***Indicates whether the UE supports *mpsPriorityIndication* on RRC release with redirect as defined in TS 38.331 [9]. | UE | No | No | No |
| ***musim-GapPreference-r17***Indicates whether the UE supports providing MUSIM assistance information with MUSIM gap preference and related MUSIM gap configuration, as defined in TS 38.331 [9]. UE supporting this feature supports 3 periodic gaps and 1 aperiodic gap. | UE | No | No | No |
| ***musimLeaveConnected-r17***Indicates whether the UE supports providing MUSIM assistance information with indication of leaving RRC\_CONNECTED state as defined in TS 38.331 [9]. | UE | No | No | No |
| ***nonTerrestrialNetwork-r17***Indicates whether the UE supports NR NTN access. If the UE indicates this capability the UE shall support the following NTN essential features, e.g., timer extension in MAC/RLC/PDCP layers and RACH adaptation to handle long RTT, acquiring NTN specific SIB and more than one TAC per PLMN broadcast in one cell. | UE | No | No | No |
| ***ntn-ScenarioSupport-r17***Indicates whether the UE supports the NTN features in GSO scenario or NGSO scenario. If a UE does not include this field but includes *nonTerrestrialNetwork-r17*, the UE supports the NTN features for both GSO and NGSO scenarios, and also supports mobility between GSO and NGSO scenarios. | UE | No | No | No |
| ***onDemandSIB-Connected-r16***Indicates whether the UE supports the on-demand request procedure of SIB(s) or posSIB(s) while in RRC\_CONNECTED, as specified in TS 38.331 [9]. | UE | No | No | No |
| ***overheatingInd***Indicates whether the UE supports overheating assistance information. | UE | No | No | No |
| ***pei-SubgroupingSupportBandList-r17***Indicates whether the UE supports receiving paging early indication in DCI format 2\_7 as specified in TS38.304 [21] for a list of frequency band. The UE shall support UEID based subgrouping for a frequency band if it indicates supporting of paging early indication reception for the frequency band. The set of OFDM symbols within a slot where UE can monitor the PEI PDCCH in Type 2A CSS is the same as the requirement for paging PDCCH in Type 2 CSS for IDLE and INACTIVE mode UEs. | UE | No | No | No |
| ***partialFR2-FallbackRX-Req***Indicates whether the UE meets only a partial set of the UE minimum receiver requirements for the eligible FR2 fallback band combinations as defined in Clause 4.2 of TS 38.101-2 [3] and Clause 4.2 of TS 38.101-3 [4]. If not indicated, the UE shall meet all the UE minimum receiver requirements for all the FR2 fallback combinations in TS 38.101-2 [3] and TS 38.101-3 [4]. The UE shall support configuration of any of the FR2 fallback band combinations regardless of the presence or the absence of this field. | UE | No | No | No |
| ***pdu-SetDiscard-r18***Indicates whether the UE supports PDU set based discard operation (i.e. *pdu-SetDiscard-r18* configuration, as specified in TS 38.331). UE supporting *pdu-SetDiscard-r18* shall also support the ability to identify PDU sets for UL XR traffic. | UE | No | No | No |
| ***psi-BasedDiscard-r18***Indicates whether the UEs supports PSI based discard (i.e. *psi-BasedDiscard-r18* configuration, as specified in TS 38.331). UE supporting *psi-BasedDiscard-r18* shall also support the ability to identify PDU sets and PSI for UL XR traffic. | UE | No | No | No |
| ***ra-SDT-r17***Indicates whether the UE supports transmission of data and/or signalling over allowed radio bearers in RRC\_INACTIVE state via Random Access procedure (i.e., RA-SDT) with 4-step RA type and if UE supports *twoStepRACH-r16,* with 2-step RA type, as specified in TS 38.331 [9]. | UE | No | No | No |
| ***ra-SDT-NTN-r17***Indicates whether the UE supports transmission of data and/or signalling over allowed radio bearers in RRC\_INACTIVE state in NTN via Random Access procedure (i.e., RA-SDT) with 4-step RA type and if UE supports *twoStepRACH-r16* for NTN*,* with 2-step RA type, as specified in TS 38.331 [9]. A UE supporting this feature shall also indicate the support of *nonTerrestrialNetwork-r17*. | UE | No | No | No |
| ***redirectAtResumeByNAS-r16***Indicates whether the UE supports reception of *redirectedCarrierInfo* in an *RRCRelease* message in response to an *RRCResumeRequest* or *RRCResumeRequest1* which is triggered by the NAS layer, as specified in TS 38.331 [9]. | UE | No | No | No |
| ***reducedCP-Latency***Indicates whether the UE supports reduced control plane latency as defined in TS 38.331 [9] | UE | No | No | No |
| ***referenceTimeProvision-r16***Indicates whether the UE supports provision of referenceTimeInfo in *DLInformationTransfer* message and in SIB9 and reference time information preference indication via assistance information, as specified in TS 38.331 [9]. | UE | No | No | No |
| ***releasePreference-r16***Indicates whether the UE supports providing its preference assistance information to transition out of RRC\_CONNECTED for power saving, as specified in TS 38.331 [9]. | UE | No | No | No |
| ***resumeWithStoredMCG-SCells-r16***Indicates whether the UE supports not deleting the stored MCG SCell configuration when initiating the resume procedure. | UE | No | No | No |
| ***resumeWithStoredSCG-r16***Indicates whether the UE supports not deleting the stored SCG configuration when initiating resume. The UE which indicates support for *resumeWithStoredSCG-r16* shall also indicate support for *resumeWithSCG-Config-r16*. | UE | No | No | No |
| ***resumeWithSCG-Config-r16***Indicates whether the UE supports (re-)configuration of an SCG during the resume procedure. | UE | No | No | No |
| ***sliceInfoforCellReselection-r17***Indicates whether the UE supports slice-based cell reselection information in SIB and on RRC release for slice-based cell reselection in RRC \_IDLE and RRC INACTIVE as defined in TS 38.304 [21]. | UE | No | No | No |
| ***splitSRB-WithOneUL-Path***Indicates whether the UE supports UL transmission via MCG path and DL reception via either MCG path or SCG path, as specified for the split SRB in TS 37.340 [7]. The UE shall not set the FDD/TDD specific fields for this capability (i.e. it shall not include this field in *UE-MRDC-CapabilityAddXDD-Mode*). | UE | No | No | No |
| ***splitDRB-withUL-Both-MCG-SCG***Indicates whether the UE supports UL transmission via both MCG path and SCG path for the split DRB as specified in TS 37.340 [7]. The UE shall not set the FDD/TDD specific fields for this capability (i.e. it shall not include this field in *UE-MRDC-CapabilityAddXDD-Mode*). | UE | Yes | No | No |
| ***srb3***Indicates whether the UE supports direct SRB between the SN and the UE as specified in TS 37.340 [7]. The UE shall not set the FDD/TDD specific fields for this capability (i.e. it shall not include this field in *UE-MRDC-CapabilityAddXDD-Mode*). This field is not applied to NE-DC. | UE | Yes | No | No |
| ***srb-SDT-NTN-r17***Indicates whether the UE supports the usage of signalling radio bearer SRB2 over RA-SDT or CG-SDT in NTN, as specified in TS 38.331 [9].A UE supporting this feature shall also indicate support of *ra-SDT-NTN-r17*, *or cg-SDT-r17* in NTN bands. A UE supporting this feature shall also indicate the support of *nonTerrestrialNetwork-r17*. | UE | No | No | No |
| ***srb-SDT-r17***Indicates whether the UE supports the usage of signalling radio bearer SRB2 over RA-SDT or CG-SDT, as specified in TS 38.331 [9].A UE supporting this feature shall also indicate support of *ra-SDT-r17 or cg-SDT-r17*. | UE | No | No | No |
| ***ul-GapFR2-Pattern-r17***Indicates FR2 UL gap pattern(s) supported by the UE for NR SA, for NR-DC without FR2-FR2 band combination, for NE-DC, and for (NG)EN-DC, if UE supports a band in FR2. The leading / leftmost bit (bit 0) corresponds to the FR2 UL gap pattern 0, the next bit corresponds to the FR2 UL gap pattern 1, as specified in TS 38.133 [5] and so on. The UE shall set at least one of the bits to 1 for FR2 UL gap pattern 1 and 3, if the UE indicates support for *ul-GapFR2-r17* in an FR2 band. | UE | CY | No | FR2 only |
| ***ul-RRC-Segmentation-r16***Indicates whether the UE supports uplink RRC segmentation of *UECapabilityInformation* as specified in TS 38.331 [9]. | UE | No | No | No |
| ***ul-TrafficInfo-r18***Indicates whether UE supports sending UE assistance information with UL traffic information such as, jitter range, burst arrival time, data burst periodicity and whether UE is able to identify PDU Set related information per UL QoS flow as specified in TS 38.331 [9].  | UE | No | No | No |

***End of the modified section***

# Annex: RAN2 UE capability feature list

According to the following agreements made in RAN2#116-e, RAN2 determined UE capabilities in the feature list format for TR 38.822 is included.

* Include an annex containing the RAN2 determined UE capabilities in the feature list format in the running UE capability CRs (similar to annex containing RAN2 agreements) for easy compilation into the TR38.822 in the later stage.
* For capabilities developed in R2, WIs will provide input to the mega CR.

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Features | Index | Feature group | Components | Prerequisite feature groups | Field name in TS 38.331 | Parent IE in TS 38.331 | Need of FDD/TDD differentiation | Need of FR1/FR2 differentiation | Note | Mandatory/Optional |
| x.NR\_XR\_enh-Core | x-1 | Additional BSR table | Indicates whether the UE supports the BSR enhancements associated with the additional BSR tables as specified in TS 38.321 [8] and 38.331 [9]. |  | *additionalBSR-Table-r18* | *UE-NR-Capability-v18xy* | No | No |  | Optional with capability signalling |
| x.NR\_XR\_enh-Core | x-2 | Delay Status Report | Indicates whether the UE supports the delay status report of the buffered data as specified in TS 38.321 [8] and 38.331 [9], 38.323 [16] and 38.322 [x]. |  | *delayStatusReport-r18* | *UE-NR-Capability-v18xy* | No | No |  | Optional with capability signalling |
| x.NR\_XR\_enh-Core | x-3 | Disable CG ReTx Monitoring | Indicates whether the UE supports to disable monitoring for retransmissions corresponding to a *ConfiguredGrantConfig* as specified in TS 38.321 [8] and 38.331 [9] |  | *disableCG-RetransmissionMonitoring -r18* | *UE-NR-Capability-v18xy* | No | No |  | Optional with capability signalling |
| x.NR\_XR\_enh-Core | x-4 | Enhanced DRX | Indicates whether the UE supports DRX enhancements including the support of non-integer DRX periodicity and addressing the SFN wrap around as specified in TS 38.331 [9] and 38.321 [8]. |  | *enhancedDRX-r18* | *UE-NR-Capability-v18xy* | No | No |  | Optional with capability signalling |
| x.NR\_XR\_enh-Core | x-5 | PDU Set based discard | Indicates whether the UEs supports PDU set based discard operation (i.e. *pdu-SetDiscard-r18* configuration, as specified in TS 38.331 [9]).  | See note | *pdu-SetDiscard-r18* | *UE-NR-Capability-v18xy* | No | No | UE supporting *pdu-SetDiscard-r18* shall also support XR awareness for UL traffic (i.e. ability to identify PDU sets, data bursts, PSI). | Optional with capability signalling |
| x.NR\_XR\_enh-Core | x-6 | PSI based discard | Indicates whether the UEs supports PSI based discard (i.e. *psi-BasedDiscard-r18* configuration, as specified in TS 38.331).  | See note | *psi-BasedDiscard-r18* | *UE-NR-Capability-v18xy* | No | No | UE supporting *psi-BasedDiscard-r18* shall also support XR awareness for UL traffic (i.e. ability to identify PDU sets, data bursts, PSI). | Optional with capability signalling |
| x.NR\_XR\_enh-Core | x-7 | UL traffic information | Indicates whether UE supports the new UE assistance information on UL traffic information to report jitter range, burst arrival time, data burst periodicity and whether UE is able to differentiate PDU Set related information per UL QoS flow as specified in TS 38.331 [9].  | See note | *ul-TrafficInfo-r18* | *UE-NR-Capability-v18xy* | No | No |  | Optional with capability signalling |