**3GPP TSG-RAN WG2 Meeting #125 *R2-24xxxxx***

**Athens, Greece, 26 February – 1 March, 2024**

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  | **38.331** | **CR** | **4445** | **rev** | **2** | **Current version:** | **18.0.0** |  |
|  |
| *For* ***[HE](http://www.3gpp.org/3G_Specs/CRs.htm%22%20%5Cl%20%22_blank)******[LP](http://www.3gpp.org/3G_Specs/CRs.htm%22%20%5Cl%20%22_blank)*** *on using this form: comprehensive instructions can be found at <http://www.3gpp.org/Change-Requests>.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network | **X** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | UE capability for Enhanced channel raster |
|  |  |
| ***Source to WG:*** | Ericsson |
| ***Source to TSG:*** | R2 |
|  |  |
| ***Work item code:*** | NR\_channel\_raster\_enh  |  | ***Date:*** | 2024-02-12 |
|  |  |  |  |  |
| ***Category:*** | **B** |  | ***Release:*** | Rel-18 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | In LS [R4-2317773](http://www.3gpp.org/ftp//tsg_ran/WG4_Radio/TSGR4_108bis/Docs//R4-2317773.zip), RAN4 indicated that a new UE capability for enhanced UE channel raster with 10 kHz granularity should be specified:* The capability should be indicated per band and be applicable for all TN and NTN FR1 bands below 3GHz with a 100 kHz channel raster.
* The capability is not applicable for bands within FR2-1/FR2-2.
* RAN4 also prefers that the capability be considered for early implementation from Rel-16.
 |
|  |  |
| ***Summary of change:*** | New capability *enhancedChannelRaster-r18* is introduced per NR band.Implementation of this CR from Rel-16 will not cause interoperability issues. |
|  |  |
| ***Consequences if not approved:*** | UE cannot indicate support of enhanced channel raster. |
|  |  |
| ***Clauses affected:*** | 6.3.3, Annex C |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** | **Y** |  |  Other core specifications  | TS 38.306 CR994r2  |
| ***affected:*** |  | **N** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **N** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** | R2-2312819, R4-2403636 |

####

### 6.3.3 UE capability information elements

<cut>

#### – *RF-Parameters*

The IE *RF-Parameters* is used to convey RF-related capabilities for NR operation.

*RF-Parameters* information element

-- ASN1START

-- TAG-RF-PARAMETERS-START

RF-Parameters ::= SEQUENCE {

 supportedBandListNR SEQUENCE (SIZE (1..maxBands)) OF BandNR,

 supportedBandCombinationList BandCombinationList OPTIONAL,

 appliedFreqBandListFilter FreqBandList OPTIONAL,

 ...,

 [[

 supportedBandCombinationList-v1540 BandCombinationList-v1540 OPTIONAL,

 srs-SwitchingTimeRequested ENUMERATED {true} OPTIONAL

 ]],

 [[

 supportedBandCombinationList-v1550 BandCombinationList-v1550 OPTIONAL

 ]],

 [[

 supportedBandCombinationList-v1560 BandCombinationList-v1560 OPTIONAL

 ]],

 [[

 supportedBandCombinationList-v1610 BandCombinationList-v1610 OPTIONAL,

 supportedBandCombinationListSidelinkEUTRA-NR-r16 BandCombinationListSidelinkEUTRA-NR-r16 OPTIONAL,

 supportedBandCombinationList-UplinkTxSwitch-r16 BandCombinationList-UplinkTxSwitch-r16 OPTIONAL

 ]],

 [[

 supportedBandCombinationList-v1630 BandCombinationList-v1630 OPTIONAL,

 supportedBandCombinationListSidelinkEUTRA-NR-v1630 BandCombinationListSidelinkEUTRA-NR-v1630 OPTIONAL,

 supportedBandCombinationList-UplinkTxSwitch-v1630 BandCombinationList-UplinkTxSwitch-v1630 OPTIONAL

 ]],

 [[

 supportedBandCombinationList-v1640 BandCombinationList-v1640 OPTIONAL,

 supportedBandCombinationList-UplinkTxSwitch-v1640 BandCombinationList-UplinkTxSwitch-v1640 OPTIONAL

 ]],

 [[

 supportedBandCombinationList-v1650 BandCombinationList-v1650 OPTIONAL,

 supportedBandCombinationList-UplinkTxSwitch-v1650 BandCombinationList-UplinkTxSwitch-v1650 OPTIONAL

 ]],

 [[

 extendedBand-n77-r16 ENUMERATED {supported} OPTIONAL

 ]],

 [[

 supportedBandCombinationList-UplinkTxSwitch-v1670 BandCombinationList-UplinkTxSwitch-v1670 OPTIONAL

 ]],

 [[

 supportedBandCombinationList-v1680 BandCombinationList-v1680 OPTIONAL

 ]],

 [[

 supportedBandCombinationList-v1690 BandCombinationList-v1690 OPTIONAL,

 supportedBandCombinationList-UplinkTxSwitch-v1690 BandCombinationList-UplinkTxSwitch-v1690 OPTIONAL

 ]],

 [[

 supportedBandCombinationList-v1700 BandCombinationList-v1700 OPTIONAL,

 supportedBandCombinationList-UplinkTxSwitch-v1700 BandCombinationList-UplinkTxSwitch-v1700 OPTIONAL,

 supportedBandCombinationListSL-RelayDiscovery-r17 OCTET STRING OPTIONAL, -- Contains PC5 BandCombinationListSidelinkNR-r16

 supportedBandCombinationListSL-NonRelayDiscovery-r17 OCTET STRING OPTIONAL, -- Contains PC5 BandCombinationListSidelinkNR-r16

 supportedBandCombinationListSidelinkEUTRA-NR-v1710 BandCombinationListSidelinkEUTRA-NR-v1710 OPTIONAL,

 sidelinkRequested-r17 ENUMERATED {true} OPTIONAL,

 extendedBand-n77-2-r17 ENUMERATED {supported} OPTIONAL

 ]],

 [[

 supportedBandCombinationList-v1720 BandCombinationList-v1720 OPTIONAL,

 supportedBandCombinationList-UplinkTxSwitch-v1720 BandCombinationList-UplinkTxSwitch-v1720 OPTIONAL

 ]],

 [[

 supportedBandCombinationList-v1730 BandCombinationList-v1730 OPTIONAL,

 supportedBandCombinationList-UplinkTxSwitch-v1730 BandCombinationList-UplinkTxSwitch-v1730 OPTIONAL,

 supportedBandCombinationListSL-RelayDiscovery-v1730 BandCombinationListSL-Discovery-r17 OPTIONAL,

 supportedBandCombinationListSL-NonRelayDiscovery-v1730 BandCombinationListSL-Discovery-r17 OPTIONAL

 ]],

 [[

 supportedBandCombinationList-v1740 BandCombinationList-v1740 OPTIONAL,

 supportedBandCombinationList-UplinkTxSwitch-v1740 BandCombinationList-UplinkTxSwitch-v1740 OPTIONAL

 ]],

 [[

 supportedBandCombinationList-v1760 BandCombinationList-v1760 OPTIONAL,

 supportedBandCombinationList-UplinkTxSwitch-v1760 BandCombinationList-UplinkTxSwitch-v1760 OPTIONAL

 ]],

 [[

 supportedBandCombinationList-v1770 BandCombinationList-v1770 OPTIONAL,

 supportedBandCombinationList-UplinkTxSwitch-v1770 BandCombinationList-UplinkTxSwitch-v1770 OPTIONAL

 ]],

 [[

 supportedBandCombinationList-v1800 BandCombinationList-v1800 OPTIONAL,

 supportedBandCombinationList-UplinkTxSwitch-v1800 BandCombinationList-UplinkTxSwitch-v1800 OPTIONAL,

 supportedBandCombinationListSL-U2U-Relay-r18 SEQUENCE {

 supportedBandCombinationListSL-U2U-RelayDiscovery-r18 OCTET STRING OPTIONAL, -- Contains PC5

 -- BandCombinationListSidelinkNR-r16

 supportedBandCombinationListSL-U2U-DiscoveryExt BandCombinationListSL-Discovery-r17 OPTIONAL

 } OPTIONAL

 ]]

}

RF-Parameters-v15g0 ::= SEQUENCE {

 supportedBandCombinationList-v15g0 BandCombinationList-v15g0 OPTIONAL

}

RF-Parameters-v16a0 ::= SEQUENCE {

 supportedBandCombinationList-v16a0 BandCombinationList-v16a0 OPTIONAL,

 supportedBandCombinationList-UplinkTxSwitch-v16a0 BandCombinationList-UplinkTxSwitch-v16a0 OPTIONAL

}

RF-Parameters-v16c0 ::= SEQUENCE {

 supportedBandListNR-v16c0 SEQUENCE (SIZE (1..maxBands)) OF BandNR-v16c0

}

BandNR ::= SEQUENCE {

 bandNR FreqBandIndicatorNR,

 modifiedMPR-Behaviour BIT STRING (SIZE (8)) OPTIONAL,

 mimo-ParametersPerBand MIMO-ParametersPerBand OPTIONAL,

 extendedCP ENUMERATED {supported} OPTIONAL,

 multipleTCI ENUMERATED {supported} OPTIONAL,

 bwp-WithoutRestriction ENUMERATED {supported} OPTIONAL,

 bwp-SameNumerology ENUMERATED {upto2, upto4} OPTIONAL,

 bwp-DiffNumerology ENUMERATED {upto4} OPTIONAL,

 crossCarrierScheduling-SameSCS ENUMERATED {supported} OPTIONAL,

 pdsch-256QAM-FR2 ENUMERATED {supported} OPTIONAL,

 pusch-256QAM ENUMERATED {supported} OPTIONAL,

 ue-PowerClass ENUMERATED {pc1, pc2, pc3, pc4} OPTIONAL,

 rateMatchingLTE-CRS ENUMERATED {supported} OPTIONAL,

 channelBWs-DL CHOICE {

 fr1 SEQUENCE {

 scs-15kHz BIT STRING (SIZE (10)) OPTIONAL,

 scs-30kHz BIT STRING (SIZE (10)) OPTIONAL,

 scs-60kHz BIT STRING (SIZE (10)) OPTIONAL

 },

 fr2 SEQUENCE {

 scs-60kHz BIT STRING (SIZE (3)) OPTIONAL,

 scs-120kHz BIT STRING (SIZE (3)) OPTIONAL

 }

 } OPTIONAL,

 channelBWs-UL CHOICE {

 fr1 SEQUENCE {

 scs-15kHz BIT STRING (SIZE (10)) OPTIONAL,

 scs-30kHz BIT STRING (SIZE (10)) OPTIONAL,

 scs-60kHz BIT STRING (SIZE (10)) OPTIONAL

 },

 fr2 SEQUENCE {

 scs-60kHz BIT STRING (SIZE (3)) OPTIONAL,

 scs-120kHz BIT STRING (SIZE (3)) OPTIONAL

 }

 } OPTIONAL,

 ...,

 [[

 maxUplinkDutyCycle-PC2-FR1 ENUMERATED {n60, n70, n80, n90, n100} OPTIONAL

 ]],

 [[

 pucch-SpatialRelInfoMAC-CE ENUMERATED {supported} OPTIONAL,

 powerBoosting-pi2BPSK ENUMERATED {supported} OPTIONAL

 ]],

 [[

 maxUplinkDutyCycle-FR2 ENUMERATED {n15, n20, n25, n30, n40, n50, n60, n70, n80, n90, n100} OPTIONAL

 ]],

 [[

 channelBWs-DL-v1590 CHOICE {

 fr1 SEQUENCE {

 scs-15kHz BIT STRING (SIZE (16)) OPTIONAL,

 scs-30kHz BIT STRING (SIZE (16)) OPTIONAL,

 scs-60kHz BIT STRING (SIZE (16)) OPTIONAL

 },

 fr2 SEQUENCE {

 scs-60kHz BIT STRING (SIZE (8)) OPTIONAL,

 scs-120kHz BIT STRING (SIZE (8)) OPTIONAL

 }

 } OPTIONAL,

 channelBWs-UL-v1590 CHOICE {

 fr1 SEQUENCE {

 scs-15kHz BIT STRING (SIZE (16)) OPTIONAL,

 scs-30kHz BIT STRING (SIZE (16)) OPTIONAL,

 scs-60kHz BIT STRING (SIZE (16)) OPTIONAL

 },

 fr2 SEQUENCE {

 scs-60kHz BIT STRING (SIZE (8)) OPTIONAL,

 scs-120kHz BIT STRING (SIZE (8)) OPTIONAL

 }

 } OPTIONAL

 ]],

 [[

 asymmetricBandwidthCombinationSet BIT STRING (SIZE (1..32)) OPTIONAL

 ]],

 [[

 -- R1 10: NR-unlicensed

 sharedSpectrumChAccessParamsPerBand-r16 SharedSpectrumChAccessParamsPerBand-r16 OPTIONAL,

 -- R1 11-7b: Independent cancellation of the overlapping PUSCHs in an intra-band UL CA

 cancelOverlappingPUSCH-r16 ENUMERATED {supported} OPTIONAL,

 -- R1 14-1: Multiple LTE-CRS rate matching patterns

 multipleRateMatchingEUTRA-CRS-r16 SEQUENCE {

 maxNumberPatterns-r16 INTEGER (2..6),

 maxNumberNon-OverlapPatterns-r16 INTEGER (1..3)

 } OPTIONAL,

 -- R1 14-1a: Two LTE-CRS overlapping rate matching patterns within a part of NR carrier using 15 kHz overlapping with a LTE carrier

 overlapRateMatchingEUTRA-CRS-r16 ENUMERATED {supported} OPTIONAL,

 -- R1 14-2: PDSCH Type B mapping of length 9 and 10 OFDM symbols

 pdsch-MappingTypeB-Alt-r16 ENUMERATED {supported} OPTIONAL,

 -- R1 14-3: One slot periodic TRS configuration for FR1

 oneSlotPeriodicTRS-r16 ENUMERATED {supported} OPTIONAL,

 olpc-SRS-Pos-r16 OLPC-SRS-Pos-r16 OPTIONAL,

 spatialRelationsSRS-Pos-r16 SpatialRelationsSRS-Pos-r16 OPTIONAL,

 simulSRS-MIMO-TransWithinBand-r16 ENUMERATED {n2} OPTIONAL,

 channelBW-DL-IAB-r16 CHOICE {

 fr1-100mhz SEQUENCE {

 scs-15kHz ENUMERATED {supported} OPTIONAL,

 scs-30kHz ENUMERATED {supported} OPTIONAL,

 scs-60kHz ENUMERATED {supported} OPTIONAL

 },

 fr2-200mhz SEQUENCE {

 scs-60kHz ENUMERATED {supported} OPTIONAL,

 scs-120kHz ENUMERATED {supported} OPTIONAL

 }

 } OPTIONAL,

 channelBW-UL-IAB-r16 CHOICE {

 fr1-100mhz SEQUENCE {

 scs-15kHz ENUMERATED {supported} OPTIONAL,

 scs-30kHz ENUMERATED {supported} OPTIONAL,

 scs-60kHz ENUMERATED {supported} OPTIONAL

 },

 fr2-200mhz SEQUENCE {

 scs-60kHz ENUMERATED {supported} OPTIONAL,

 scs-120kHz ENUMERATED {supported} OPTIONAL

 }

 } OPTIONAL,

 rasterShift7dot5-IAB-r16 ENUMERATED {supported} OPTIONAL,

 ue-PowerClass-v1610 ENUMERATED {pc1dot5} OPTIONAL,

 condHandover-r16 ENUMERATED {supported} OPTIONAL,

 condHandoverFailure-r16 ENUMERATED {supported} OPTIONAL,

 condHandoverTwoTriggerEvents-r16 ENUMERATED {supported} OPTIONAL,

 condPSCellChange-r16 ENUMERATED {supported} OPTIONAL,

 condPSCellChangeTwoTriggerEvents-r16 ENUMERATED {supported} OPTIONAL,

 mpr-PowerBoost-FR2-r16 ENUMERATED {supported} OPTIONAL,

 -- R1 11-9: Multiple active configured grant configurations for a BWP of a serving cell

 activeConfiguredGrant-r16 SEQUENCE {

 maxNumberConfigsPerBWP-r16 ENUMERATED {n1, n2, n4, n8, n12},

 maxNumberConfigsAllCC-r16 INTEGER (2..32)

 } OPTIONAL,

 -- R1 11-9a: Joint release in a DCI for two or more configured grant Type 2 configurations for a given BWP of a serving cell

 jointReleaseConfiguredGrantType2-r16 ENUMERATED {supported} OPTIONAL,

 -- R1 12-2: Multiple SPS configurations

 sps-r16 SEQUENCE {

 maxNumberConfigsPerBWP-r16 INTEGER (1..8),

 maxNumberConfigsAllCC-r16 INTEGER (2..32)

 } OPTIONAL,

 -- R1 12-2a: Joint release in a DCI for two or more SPS configurations for a given BWP of a serving cell

 jointReleaseSPS-r16 ENUMERATED {supported} OPTIONAL,

 -- R1 13-19: Simultaneous positioning SRS and MIMO SRS transmission within a band across multiple CCs

 simulSRS-TransWithinBand-r16 ENUMERATED {n2} OPTIONAL,

 trs-AdditionalBandwidth-r16 ENUMERATED {trs-AddBW-Set1, trs-AddBW-Set2} OPTIONAL,

 handoverIntraF-IAB-r16 ENUMERATED {supported} OPTIONAL

 ]],

 [[

 -- R1 22-5a: Simultaneous transmission of SRS for antenna switching and SRS for CB/NCB /BM for intra-band UL CA

 -- R1 22-5c: Simultaneous transmission of SRS for antenna switching and SRS for antenna switching for intra-band UL CA

 simulTX-SRS-AntSwitchingIntraBandUL-CA-r16 SimulSRS-ForAntennaSwitching-r16 OPTIONAL,

 -- R1 10: NR-unlicensed

 sharedSpectrumChAccessParamsPerBand-v1630 SharedSpectrumChAccessParamsPerBand-v1630 OPTIONAL

 ]],

 [[

 handoverUTRA-FDD-r16 ENUMERATED {supported} OPTIONAL,

 -- R4 7-4: Report the shorter transient capability supported by the UE: 2, 4 or 7us

 enhancedUL-TransientPeriod-r16 ENUMERATED {us2, us4, us7} OPTIONAL,

 sharedSpectrumChAccessParamsPerBand-v1640 SharedSpectrumChAccessParamsPerBand-v1640 OPTIONAL

 ]],

 [[

 type1-PUSCH-RepetitionMultiSlots-v1650 ENUMERATED {supported} OPTIONAL,

 type2-PUSCH-RepetitionMultiSlots-v1650 ENUMERATED {supported} OPTIONAL,

 pusch-RepetitionMultiSlots-v1650 ENUMERATED {supported} OPTIONAL,

 configuredUL-GrantType1-v1650 ENUMERATED {supported} OPTIONAL,

 configuredUL-GrantType2-v1650 ENUMERATED {supported} OPTIONAL,

 sharedSpectrumChAccessParamsPerBand-v1650 SharedSpectrumChAccessParamsPerBand-v1650 OPTIONAL

 ]],

 [[

 enhancedSkipUplinkTxConfigured-v1660 ENUMERATED {supported} OPTIONAL,

 enhancedSkipUplinkTxDynamic-v1660 ENUMERATED {supported} OPTIONAL

 ]],

 [[

 maxUplinkDutyCycle-PC1dot5-MPE-FR1-r16 ENUMERATED {n10, n15, n20, n25, n30, n40, n50, n60, n70, n80, n90, n100} OPTIONAL,

 txDiversity-r16 ENUMERATED {supported} OPTIONAL

 ]],

 [[

 -- R1 36-1: Support of 1024QAM for PDSCH for FR1

 pdsch-1024QAM-FR1-r17 ENUMERATED {supported} OPTIONAL,

 -- R4 22-1 support of FR2 HST operation

 ue-PowerClass-v1700 ENUMERATED {pc5, pc6, pc7} OPTIONAL,

 -- R1 24: NR extension to 71GHz (FR2-2)

 fr2-2-AccessParamsPerBand-r17 FR2-2-AccessParamsPerBand-r17 OPTIONAL,

 rlm-Relaxation-r17 ENUMERATED {supported} OPTIONAL,

 bfd-Relaxation-r17 ENUMERATED {supported} OPTIONAL,

 cg-SDT-r17 ENUMERATED {supported} OPTIONAL,

 locationBasedCondHandover-r17 ENUMERATED {supported} OPTIONAL,

 timeBasedCondHandover-r17 ENUMERATED {supported} OPTIONAL,

 eventA4BasedCondHandover-r17 ENUMERATED {supported} OPTIONAL,

 mn-InitiatedCondPSCellChangeNRDC-r17 ENUMERATED {supported} OPTIONAL,

 sn-InitiatedCondPSCellChangeNRDC-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 29-3a: PDCCH skipping

 pdcch-SkippingWithoutSSSG-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 29-3b: 2 search space sets group switching

 sssg-Switching-1BitInd-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 29-3c: 3 search space sets group switching

 sssg-Switching-2BitInd-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 29-3d: 2 search space sets group switching with PDCCH skipping

 pdcch-SkippingWithSSSG-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 29-3e: Support Search space set group switching capability 2 for FR1

 searchSpaceSetGrp-switchCap2-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 26-1: Uplink Time and Frequency pre-compensation and timing relationship enhancements

 uplinkPreCompensation-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 26-4: UE reporting of information related to TA pre-compensation

 uplink-TA-Reporting-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 26-5: Increasing the number of HARQ processes

 max-HARQ-ProcessNumber-r17 ENUMERATED {u16d32, u32d16, u32d32} OPTIONAL,

 -- R1 26-6: Type-2 HARQ codebook enhancement

 type2-HARQ-Codebook-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 26-6a: Type-1 HARQ codebook enhancement

 type1-HARQ-Codebook-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 26-6b: Type-3 HARQ codebook enhancement

 type3-HARQ-Codebook-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 26-9: UE-specific K\_offset

 ue-specific-K-Offset-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 24-1f: Multiple PDSCH scheduling by single DCI for 120kHz in FR2-1

 multiPDSCH-SingleDCI-FR2-1-SCS-120kHz-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 24-1g: Multiple PUSCH scheduling by single DCI for 120kHz in FR2-1

 multiPUSCH-SingleDCI-FR2-1-SCS-120kHz-r17 ENUMERATED {supported} OPTIONAL,

 -- R4 14-4: Parallel PRS measurements in RRC\_INACTIVE state, FR1/FR2 diff

 parallelPRS-MeasRRC-Inactive-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 27-1-2: Support of UE-TxTEGs for UL TDOA

 nr-UE-TxTEG-ID-MaxSupport-r17 ENUMERATED {n1, n2, n3, n4, n6, n8} OPTIONAL,

 -- R1 27-17: PRS processing in RRC\_INACTIVE

 prs-ProcessingRRC-Inactive-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 27-3-2: DL PRS measurement outside MG and in a PRS processing window

 prs-ProcessingWindowType1A-r17 ENUMERATED {option1, option2, option3} OPTIONAL,

 prs-ProcessingWindowType1B-r17 ENUMERATED {option1, option2, option3} OPTIONAL,

 prs-ProcessingWindowType2-r17 ENUMERATED {option1, option2, option3} OPTIONAL,

 -- R1 27-15: Positioning SRS transmission in RRC\_INACTIVE state for initial UL BWP

 srs-AllPosResourcesRRC-Inactive-r17 SRS-AllPosResourcesRRC-Inactive-r17 OPTIONAL,

 -- R1 27-16: OLPC for positioning SRS in RRC\_INACTIVE state - gNB

 olpc-SRS-PosRRC-Inactive-r17 OLPC-SRS-Pos-r16 OPTIONAL,

 -- R1 27-19: Spatial relation for positioning SRS in RRC\_INACTIVE state - gNB

 spatialRelationsSRS-PosRRC-Inactive-r17 SpatialRelationsSRS-Pos-r16 OPTIONAL,

 -- R1 30-1: Increased maximum number of PUSCH Type A repetitions

 maxNumberPUSCH-TypeA-Repetition-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 30-2: PUSCH Type A repetitions based on available slots

 puschTypeA-RepetitionsAvailSlot-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 30-3: TB processing over multi-slot PUSCH

 tb-ProcessingMultiSlotPUSCH-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 30-3a: Repetition of TB processing over multi-slot PUSCH

 tb-ProcessingRepMultiSlotPUSCH-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 30-4: The maximum duration for DM-RS bundling

 maxDurationDMRS-Bundling-r17 SEQUENCE {

 fdd-r17 ENUMERATED {n4, n8, n16, n32} OPTIONAL,

 tdd-r17 ENUMERATED {n2, n4, n8, n16} OPTIONAL

 } OPTIONAL,

 -- R1 30-6: Repetition of PUSCH transmission scheduled by RAR UL grant and DCI format 0\_0 with CRC scrambled by TC-RNTI

 pusch-RepetitionMsg3-r17 ENUMERATED {supported} OPTIONAL,

 sharedSpectrumChAccessParamsPerBand-v1710 SharedSpectrumChAccessParamsPerBand-v1710 OPTIONAL,

 -- R4 25-2: Parallel measurements on cells belonging to a different NGSO satellite than a serving satellite without scheduling restrictions

 -- on normal operations with the serving cell

 parallelMeasurementWithoutRestriction-r17 ENUMERATED {supported} OPTIONAL,

 -- R4 25-5: Parallel measurements on multiple NGSO satellites within a SMTC

 maxNumber-NGSO-SatellitesWithinOneSMTC-r17 ENUMERATED {n1, n2, n3, n4} OPTIONAL,

 -- R1 26-10: K1 range extension

 k1-RangeExtension-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 35-1: Aperiodic CSI-RS for tracking for fast SCell activation

 aperiodicCSI-RS-FastScellActivation-r17 SEQUENCE {

 maxNumberAperiodicCSI-RS-PerCC-r17 ENUMERATED {n8, n16, n32, n48, n64, n128, n255},

 maxNumberAperiodicCSI-RS-AcrossCCs-r17 ENUMERATED {n8, n16, n32, n64, n128, n256, n512, n1024}

 } OPTIONAL,

 -- R1 35-2: Aperiodic CSI-RS bandwidth for tracking for fast SCell activation for 10MHz UE channel bandwidth

 aperiodicCSI-RS-AdditionalBandwidth-r17 ENUMERATED {addBW-Set1, addBW-Set2} OPTIONAL,

 -- R1 28-1a: RRC-configured DL BWP without CD-SSB or NCD-SSB

 bwp-WithoutCD-SSB-OrNCD-SSB-RedCap-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 28-3: Half-duplex FDD operation type A for (e)RedCap UE

 halfDuplexFDD-TypeA-RedCap-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 27-15b: Positioning SRS transmission in RRC\_INACTIVE state configured outside initial UL BWP

 posSRS-RRC-Inactive-OutsideInitialUL-BWP-r17 PosSRS-RRC-Inactive-OutsideInitialUL-BWP-r17 OPTIONAL,

 -- R4 15-3 UE support of CBW for 480kHz SCS

 channelBWs-DL-SCS-480kHz-FR2-2-r17 BIT STRING (SIZE (8)) OPTIONAL,

 channelBWs-UL-SCS-480kHz-FR2-2-r17 BIT STRING (SIZE (8)) OPTIONAL,

 -- R4 15-4 UE support of CBW for 960kHz SCS

 channelBWs-DL-SCS-960kHz-FR2-2-r17 BIT STRING (SIZE (8)) OPTIONAL,

 channelBWs-UL-SCS-960kHz-FR2-2-r17 BIT STRING (SIZE (8)) OPTIONAL,

 -- R4 17-1 UL gap for Tx power management

 ul-GapFR2-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 25-4: One-shot HARQ ACK feedback triggered by DCI format 1\_2

 oneShotHARQ-feedbackTriggeredByDCI-1-2-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 25-5: PHY priority handling for one-shot HARQ ACK feedback

 oneShotHARQ-feedbackPhy-Priority-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 25-6: Enhanced type 3 HARQ-ACK codebook feedback

 enhancedType3-HARQ-CodebookFeedback-r17 SEQUENCE {

 enhancedType3-HARQ-Codebooks-r17 ENUMERATED {n1, n2, n4, n8},

 maxNumberPUCCH-Transmissions-r17 ENUMERATED {n1, n2, n3, n4, n5, n6, n7}

 } OPTIONAL,

 -- R1 25-7: Triggered HARQ-ACK codebook re-transmission

 triggeredHARQ-CodebookRetx-r17 SEQUENCE {

 minHARQ-Retx-Offset-r17 ENUMERATED {n-7, n-5, n-3, n-1, n1},

 maxHARQ-Retx-Offset-r17 ENUMERATED {n4, n6, n8, n10, n12, n14, n16, n18, n20, n22, n24}

 } OPTIONAL

 ]],

 [[

 -- R4 22-2 support of one shot large UL timing adjustment

 ue-OneShotUL-TimingAdj-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 25-2: Repetitions for PUCCH format 0, and 2 over multiple slots with K = 2, 4, 8

 pucch-Repetition-F0-2-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 25-11a: 4-bits subband CQI for NTN and unlicensed

 cqi-4-BitsSubbandNTN-SharedSpectrumChAccess-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 25-16: HARQ-ACK with different priorities multiplexing on a PUCCH/PUSCH

 mux-HARQ-ACK-DiffPriorities-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 25-20a: Propagation delay compensation based on Rel-15 TA procedure for NTN and unlicensed

 ta-BasedPDC-NTN-SharedSpectrumChAccess-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 33-2b: DCI-based enabling/disabling ACK/NACK-based feedback for dynamic scheduling for multicast

 ack-NACK-FeedbackForMulticastWithDCI-Enabler-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 33-2e: Multiple G-RNTIs for group-common PDSCHs

 maxNumberG-RNTI-r17 INTEGER (2..8) OPTIONAL,

 -- R1 33-2f: Dynamic multicast with DCI format 4\_2

 dynamicMulticastDCI-Format4-2-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 33-2i: Supported maximal modulation order for multicast PDSCH

 maxModulationOrderForMulticast-r17 CHOICE {

 fr1-r17 ENUMERATED {qam256, qam1024},

 fr2-r17 ENUMERATED {qam64, qam256}

 } OPTIONAL,

 -- R1 33-3-1: Dynamic Slot-level repetition for group-common PDSCH for TN and licensed

 dynamicSlotRepetitionMulticastTN-NonSharedSpectrumChAccess-r17 ENUMERATED {n8, n16} OPTIONAL,

 -- R1 33-3-1a: Dynamic Slot-level repetition for group-common PDSCH for NTN and unlicensed

 dynamicSlotRepetitionMulticastNTN-SharedSpectrumChAccess-r17 ENUMERATED {n8, n16} OPTIONAL,

 -- R1 33-4-1: DCI-based enabling/disabling NACK-only based feedback for dynamic scheduling for multicast

 nack-OnlyFeedbackForMulticastWithDCI-Enabler-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 33-5-1b: DCI-based enabling/disabling ACK/NACK-based feedback for dynamic scheduling for multicast

 ack-NACK-FeedbackForSPS-MulticastWithDCI-Enabler-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 33-5-1h: Multiple G-CS-RNTIs for SPS group-common PDSCHs

 maxNumberG-CS-RNTI-r17 INTEGER (2..8) OPTIONAL,

 -- R1 33-10: Support group-common PDSCH RE-level rate matching for multicast

 re-LevelRateMatchingForMulticast-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 36-1a: Support of 1024QAM for PDSCH with maximum 2 MIMO layers for FR1

 pdsch-1024QAM-2MIMO-FR1-r17 ENUMERATED {supported} OPTIONAL,

 -- R4 14-3 PRS measurement without MG

 prs-MeasurementWithoutMG-r17 ENUMERATED {cpLength, quarterSymbol, halfSymbol, halfSlot} OPTIONAL,

 -- R4 25-7: The number of target LEO satellites the UE can monitor per carrier

 maxNumber-LEO-SatellitesPerCarrier-r17 INTEGER (3..4) OPTIONAL,

 -- R1 27-3-3 DL PRS Processing Capability outside MG - buffering capability

 prs-ProcessingCapabilityOutsideMGinPPW-r17 SEQUENCE (SIZE(1..3)) OF PRS-ProcessingCapabilityOutsideMGinPPWperType-r17 OPTIONAL,

 -- R1 27-15a: Positioning SRS transmission in RRC\_INACTIVE state for initial UL BWP with semi-persistent SRS

 srs-SemiPersistent-PosResourcesRRC-Inactive-r17 SEQUENCE {

 maxNumOfSemiPersistentSRSposResources-r17 ENUMERATED {n1, n2, n4, n8, n16, n32, n64},

 maxNumOfSemiPersistentSRSposResourcesPerSlot-r17 ENUMERATED {n1, n2, n3, n4, n5, n6, n8, n10, n12, n14}

 } OPTIONAL,

 -- R2: UE support of CBW for 120kHz SCS

 channelBWs-DL-SCS-120kHz-FR2-2-r17 BIT STRING (SIZE (8)) OPTIONAL,

 channelBWs-UL-SCS-120kHz-FR2-2-r17 BIT STRING (SIZE (8)) OPTIONAL

 ]],

 [[

 -- R1 30-4a: DM-RS bundling for PUSCH repetition type A

 dmrs-BundlingPUSCH-RepTypeA-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 30-4b: DM-RS bundling for PUSCH repetition type B

 dmrs-BundlingPUSCH-RepTypeB-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 30-4c: DM-RS bundling for TB processing over multi-slot PUSCH

 dmrs-BundlingPUSCH-multiSlot-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 30-4d: DMRS bundling for PUCCH repetitions

 dmrs-BundlingPUCCH-Rep-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 30-4e: Enhanced inter-slot frequency hopping with inter-slot bundling for PUSCH

 interSlotFreqHopInterSlotBundlingPUSCH-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 30-4f: Enhanced inter-slot frequency hopping for PUCCH repetitions with DMRS bundling

 interSlotFreqHopPUCCH-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 30-4g: Restart DM-RS bundling

 dmrs-BundlingRestart-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 30-4h: DM-RS bundling for non-back-to-back transmission

 dmrs-BundlingNonBackToBackTX-r17 ENUMERATED {supported} OPTIONAL

 ]],

 [[

 -- R1 33-5-1e: Dynamic Slot-level repetition for SPS group-common PDSCH for multicast

 maxDynamicSlotRepetitionForSPS-Multicast-r17 ENUMERATED {n8, n16} OPTIONAL,

 -- R1 33-5-1g: DCI-based enabling/disabling NACK-only based feedback for SPS group-common PDSCH for multicast

 nack-OnlyFeedbackForSPS-MulticastWithDCI-Enabler-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 33-5-1i: Multicast SPS scheduling with DCI format 4\_2

 sps-MulticastDCI-Format4-2-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 33-5-2: Multiple SPS group-common PDSCH configuration on PCell

 sps-MulticastMultiConfig-r17 INTEGER (1..8) OPTIONAL,

 -- R1 33-6-1: DL priority indication for multicast in DCI

 priorityIndicatorInDCI-Multicast-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 33-6-1a: DL priority configuration for SPS multicast

 priorityIndicatorInDCI-SPS-Multicast-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 33-6-2: Two HARQ-ACK codebooks simultaneously constructed for supporting HARQ-ACK codebooks with different priorities

 -- for unicast and multicast at a UE

 twoHARQ-ACK-CodebookForUnicastAndMulticast-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 33-6-3: More than one PUCCH for HARQ-ACK transmission for multicast or for unicast and multicast within a slot

 multiPUCCH-HARQ-ACK-ForMulticastUnicast-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 33-9: Supporting unicast PDCCH to release SPS group-common PDSCH

 releaseSPS-MulticastWithCS-RNTI-r17 ENUMERATED {supported} OPTIONAL

 ]],

 [[

 -- R1 41-3-1a UE automomous TA adjustment when cell-reselection happens

 posUE-TA-AutoAdjustment-r18 ENUMERATED {supported} OPTIONAL,

 -- R1 41-4-6a support a Rel-17 single DCI scheduling positioning SRS resource sets across the linked carriers

 -- for SRS bandwidth aggregation in RRC\_CONNECTED state

 posJointTriggerBySingleDCI-RRC-Connected-r18 ENUMERATED {supported} OPTIONAL,

 -- R1 41-5-1a PRS measurement with Rx frequency hopping in RRC\_INACTIVE for RedCap UEs

 dl-PRS-MeasurementWithRxFH-RRC-InactiveforRedCap-r18 ENUMERATED {supported} OPTIONAL,

 -- R1 41-5-1b PRS measurement with Rx frequency hopping in RRC\_IDLE for RedCap UEs

 dl-PRS-MeasurementWithRxFH-RRC-IdleforRedCap-r18 ENUMERATED {supported} OPTIONAL,

 -- R1 42-4: Cell DTX and/or DRX operation based on RRC configuration

 nes-CellDTX-DRX-r18 ENUMERATED {cellDTXonly, cellDRXonly, both} OPTIONAL,

 -- R1 42-5: Cell DTX/DRX operation triggered by DCI format 2\_9

 nes-CellDTX-DRX-DCI2-9-r18 ENUMERATED {supported} OPTIONAL,

 -- R1 45-6: UE-based TA measurement

 ue-TA-Measurement-r18 INTEGER (1..8) OPTIONAL,

 -- R1 45-7: TA indication in cell switch command

 ta-IndicationCellSwitch-r18 ENUMERATED {supported} OPTIONAL,

 -- R1 50-1: Multi-PUSCHs for Configured Grant

 multiPUSCH-CG-r18 ENUMERATED {n16, n32} OPTIONAL,

 -- R1 50-1a: Multiple active multi-PUSCHs configured grant configurations for a BWP of a serving cell

 multiPUSCH-ActiveConfiguredGrant-r18 SEQUENCE {

 maxNumberConfigsPerBWP ENUMERATED {n1, n2, n4, n8, n12},

 maxNumberConfigsAllCC-FR1 INTEGER (2..32),

 maxNumberConfigsAllCC-FR2 INTEGER (2..32)

 } OPTIONAL,

 -- R1 50-2: UCI indication of unused CG-PUSCH transmission occasions

 cg-PUSCH-UTO-UCI-Ind-r18 ENUMERATED {supported} OPTIONAL,

 -- R1 50-3: PDCCH monitoring resumption after UL NACK

 pdcch-MonitoringResumptionAfterUL-NACK-r18 ENUMERATED {supported} OPTIONAL,

 -- R1 51-1: support for 3MHz channel bandwidth

 support-3MHz-ChannelBW-r18 ENUMERATED {supported} OPTIONAL,

 -- R1 51-2: support 12 PRB CORESET0

 support-12PRB-CORESET0-r18 ENUMERATED {supported} OPTIONAL,

 -- R1 52-1: Reception of NR PDCCH candidates overlapping with LTE CRS REs

 nr-PDCCH-OverlapLTE-CRS-RE-r18 SEQUENCE {

 overlapInRE-r18 ENUMERATED {oneSymbolNoOverlap, someOrAllSymOverlap},

 overlapInSymbol-r18 ENUMERATED {symbol2,symbol1And2}

 } OPTIONAL,

 -- Editor's Note: someOrAllSymOverlap considers to be supported in overlapInRE-r18 only if RAN4 performance requirements for

 -- someOrAllSymOverlap are not defined

 -- R1 52-1a: Reception of NR PDCCH candidates overlapping with LTE CRS REs with multiple non-overlapping CRS rate matching patterns

 nr-PDCCH-OverlapLTE-CRS-RE-MultiPatterns-r18 ENUMERATED {supported} OPTIONAL,

 -- R1 52-1b: NR PDCCH reception that overlaps with LTE CRS within a single span of 3 consecutive OFDM symbols that is within the

 -- first 4 OFDM symbols in a slot

 nr-PDCCH-OverlapLTE-CRS-RE-Span-3-4-r18 ENUMERATED {supported} OPTIONAL,

 -- R1 52-2: Two LTE-CRS overlapping rate matching patterns within NR 15 kHz carrier overlapping with LTE carrier (regardless of

 -- support or configuration of multi-TRP)

 twoRateMatchingEUTRA-CRS-patterns-3-4-r18 SEQUENCE {

 maxNumberPatterns-r18 INTEGER (2..6),

 maxNumberNon-OverlapPatterns-r18 INTEGER (1..3)

 } OPTIONAL,

 -- R1 52-2a: Two LTE-CRS overlapping rate matching patterns with two different values of coresetPoolIndex within NR 15 kHz carrier

 -- overlapping with LTE carrier

 overlapRateMatchingEUTRA-CRS-Patterns-3-4-Diff-CS-Pool-r18 ENUMERATED {supported} OPTIONAL,

 -- R1 53-3: Support RLM/BM/BFD measurements based on NCD-SSB within active BWP

 ncd-SSB-BWP-Wor-r18 ENUMERATED {supported} OPTIONAL,

 -- R1 53-4: Support Support RLM/BM/BFD measurements based on CSI-RS when CD-SSB is outside active BWP

 rlm-BM-BFD-CSI-RS-OutsideActiveBWP-r18 ENUMERATED {supported} OPTIONAL,

 -- R1 55-3: Multiple PUSCHs scheduling by single DCI for non-consecutive slots in FR1

 multiPUSCH-SingleDCI-NonConsSlots-r18 ENUMERATED {supported} OPTIONAL,

 -- R1 55-2d: single-symbol DL-PRS used in RTT-based Propagation delay compensation

 pdc-maxNumberPRS-ResourceProcessedPerSlot-r18 SEQUENCE {

 fr1-r18 SEQUENCE {

 scs-15kHz-r18 ENUMERATED {n1, n2, n4, n6, n8, n12, n16, n24, n32, n48, n64} OPTIONAL,

 scs-30kHz-r18 ENUMERATED {n1, n2, n4, n6, n8, n12, n16, n24, n32, n48, n64} OPTIONAL,

 scs-60kHz-r18 ENUMERATED {n1, n2, n4, n6, n8, n12, n16, n24, n32, n48, n64} OPTIONAL

 },

 fr2-r18 SEQUENCE {

 scs-60kHz-r18 ENUMERATED {n1, n2, n4, n6, n8, n12, n16, n24, n32, n48, n64} OPTIONAL,

 scs-120kHz-r18 ENUMERATED {n1, n2, n4, n6, n8, n12, n16, n24, n32, n48, n64} OPTIONAL

 }

 } OPTIONAL,

 -- R4 27-2: LowerMSD for inter-band NR CA and EN-DC

 lowerMSD-r18 SEQUENCE (SIZE (1..maxLowerMSD-r18)) OF LowerMSD-r18 OPTIONAL,

 -- R4 28-1: Enhanced channel raster

 enhancedChannelRaster-r18 ENUMERATED {supported} OPTIONAL,

 -- R4 31-2 Beam sweeping factor reduction for FR2 unknown SCell activation

 beamSweepingFactorReduction-r18 SEQUENCE {

 reduceForCellDetection ENUMERATED {n1, n2, n4, n6},

 reduceForSSB-L1-RSRP-Meas INTEGER (0..7)

 } OPTIONAL,

 -- R4 35-2: the requirements defined for ATG UE with antenna array or omni-direction antenna requirements.

 antennaArrayType-r18 ENUMERATED {supported} OPTIONAL,

 locationBasedCondHandoverATG-r18 ENUMERATED {supported} OPTIONAL,

 -- R4 35-3: rated maximum output power value range from 23dBm to 40dBm with 1dB as granularity at maximum modulation order and full

 -- PRB configurations.

 maxOutputPowerATG-r18 INTEGER (1..18) OPTIONAL,

 eventA4BasedCondHandoverNES-r18 ENUMERATED {supported} OPTIONAL,

 nesBasedCondHandoverWithDCI-r18 ENUMERATED {supported} OPTIONAL,

 rachLessHandoverNTN-r18 ENUMERATED {supported} OPTIONAL,

 locationBasedCondHandoverEMC-r18 ENUMERATED {supported} OPTIONAL,

 mt-CG-SDT-r18 ENUMERATED {supported} OPTIONAL,

 posSRS-RRC-InactiveInitialUL-BWP-r18 ENUMERATED {supported} OPTIONAL,

 posSRS-RRC-InactiveOutsideInitialUL-BWP-r18 ENUMERATED {supported} OPTIONAL,

 cg-SDT-PeriodicityExt-r18 ENUMERATED {supported} OPTIONAL

 ]]

}

BandNR-v16c0 ::= SEQUENCE {

 pusch-RepetitionTypeA-v16c0 ENUMERATED {supported} OPTIONAL,

 ...

}

LowerMSD-r18 ::= SEQUENCE {

 aggressorband1-r18 FreqBandIndicatorNR,

 aggressorband2-r18 FreqBandIndicatorNR OPTIONAL,

 msd-Information-r18 SEQUENCE (SIZE (1..maxLowerMSDInfo-r18)) OF MSD-Information-r18

}

MSD-Information-r18 ::= SEQUENCE {

 msd-Type-r18 ENUMERATED {harmonic, harmonicMixing, crossBandIsolation, imd2, imd3, imd4, imd5, all, spare8, spare7,

 spare6, spare5,spare4, spare3, spare2, spare1},

 msd-PowerClass-r18 ENUMERATED {pc1dot5, pc2, pc3},

 msd-Class-r18 ENUMERATED {classI, classII, classIII, classIV, classV, classVI, classVII, classVIII }

}

-- Editor note: The power class related part can be updated further pending RAN4 discussion.

-- TAG-RF-PARAMETERS-STOP

-- ASN1STOP

|  |
| --- |
| *RF-Parameters* field descriptions |
| ***appliedFreqBandListFilter***In this field the UE mirrors the *FreqBandList* that the NW provided in the capability enquiry, if any, as described in clause 5.6.1.4. The UE filtered the band combinations in the *supportedBandCombinationList* in accordance with this *appliedFreqBandListFilter*. The UE does not include this field if the UE capability is requested by E-UTRAN and the network request includes the field *eutra-nr-only* [10]. |
| ***supportedBandCombinationList***A list of band combinations that the UE supports for NR (and NR-DC, if requested). The *FeatureSetCombinationId*:s in this list refer to the *FeatureSetCombination* entries in the *featureSetCombinations* list in the *UE-NR-Capability* IE. The UE does not include this field if the UE capability is requested by E-UTRAN and the network request includes the field *eutra-nr-only* [10]. |
| ***supportedBandCombinationListSidelinkEUTRA-NR***A list of band combinations that the UE supports for NR sidelink communication only, for joint NR sidelink communication and V2X sidelink communication, or for V2X sidelink communication only. The UE does not include this field if the UE capability is requested by E-UTRAN (see TS 36.331[10]) and the network request includes the field *eutra-nr-only*. |
| ***supportedBandCombinationListSL-NonRelayDiscovery***A list of band combinations that the UE supports for NR sidelink non-relay discovery. The encoding is defined in PC5 *BandCombinationListSidelinkNR-r16.* |
| ***supportedBandCombinationListSL-RelayDiscovery***A list of band combinations that the UE supports for NR sidelink relay discovery. The encoding is defined in PC5 *BandCombinationListSidelinkNR-r16.* |
| ***supportedBandCombinationListSL-U2U-DiscoveryExt***This field indicates the band parameter in *BandCombinationListSL-Discovery-r17* that the UE supports for NR U2U sidelink relay discovery in a band included in *supportedBandCombinationListSL-U2U-RelayDiscovery*. |
| ***supportedBandCombinationListSL-U2U-RelayDiscovery***A list of band combinations that the UE supports for NR U2U sidelink relay discovery. The encoding is defined in PC5 *BandCombinationListSidelinkNR-r16.* |
| ***supportedBandCombinationList-UplinkTxSwitch***A list of band combinations that the UE supports dynamic uplink Tx switching for NR UL CA and SUL. The *FeatureSetCombinationId*:s in this list refer to the *FeatureSetCombination* entries in the *featureSetCombinations* list in the *UE-NR-Capability* IE. The UE does not include this field if the UE capability is requested by E-UTRAN and the network request includes the field *eutra-nr-only* [10]. |
| ***supportedBandListNR***A list of NR bands supported by the UE. If *supportedBandListNR-v16c0* is included, the UE shall include the same number of entries, and listed in the same order, as in *supportedBandListNR* (without suffix). |

Annex C (normative): List of CRs Containing Early Implementable Features and Corrections

This annex lists the Change Requests (CRs) whose changes may be implemented by a UE of an earlier release than which the CR was approved in (i.e. CRs that contain on their coversheets the sentence "Implementation of this CR from Rel-N will not cause interoperability issues").

Table C-1: List of CRs Containing Early Implementable Features and Corrections

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| TDoc Number (RP-xxxxxx): CR Title | CR Number(s) | CR Revision Number(s) | Earliest Implementable Release | Additional Information |
| RP-200335: Correction on usage of access category 2 for UAC for RNA update | 1141 | 2 | Release 15 |  |
| RP-201185: Introduction of signalling for high-speed train scenarios | 1464 | 5 | Release 15 |  |
| RP-201216: Release-16 UE capabilities based on RAN1, RAN4 feature lists and RAN2 | 1665 | 2 | Release 15 | Early implementation part is referring to the aspect covered by- R2-2006203: Extension of CSI-RS capabilities per codebook type- R2-2006360: Intraband EN\_DC power class expansion for 29 dBm |
| RP-202768: UE behaviour when UL 7.5KHz shift is not supported | 2107 | 2 | Release 15 |  |
| RP-202790: Correction on uac-AccessCategory1-SelectionAssistanceInfo | 2130 | 1 | Release 15 |  |
| RP-211483: Clarification on the initiation of RNA update | 2581 | 1 | Release 15 |  |
| RP-201190: Introduction of eCall over IMS for NR | 1670 | - | Release 15 |  |
| RP-212598: Distinguishing support of extended band n77 | 2810 | 2 | Release 15 |  |
| RP-213342: Duty cycle signalling for power class 1.5 | 2817 | 1 | Release 15 |  |
| RP-213345: CR on 38.331 for introducing UE capability of txDiversity | 2859 | 1 | Release 15 |  |
| RP-220497: Introduction of function for RRM enhancements for Rel-17 NR FR1 HST | 2898 | 2 | Release 16 |  |
| RP-220838: Release-17 UE capabilities based on R1 and R4 feature lists (TS38.331) | 2901 | 1 | Release 15 | Early implementation part is referring to the aspect covered by:- R2-2203898: Introduction of BCS4 and BCS5- R2-2203836: Introducing UE capability for power class 5 for FR2 FWA |
| RP-221721: CR on the CBM/IBM reporting-38331 | 2916 | 2 | Release 16 |  |
| RP-221736: Distinguishing support of band n77 restrictions in Canada [n77 Canada] | 3078 | 2 | Release 15 |  |
| RP-222527: Correction to additionalSpectrumEmission for UL CA in n77 for the US | 3476 | - | Release 15 |  |
| RP-222527: Correction to additionalSpectrumEmission for UL CA in n77 for Canada | 3478 | - | Release 15 |  |
| RP-232570: Addition of extended number range for NS value | 3900 | 6 | Release 16 |  |
| RP-233888: Introduction of FR2 FBG2 CA BW classes | 2867 | 6 | Release 15 |  |
| RP-233882: Enhancing SCell A2 event reporting | 4375 | 2 | Release 15 |  |
| RP-233890: PTM retransmission reception for multicast DRX with HARQ feedback disabled [PTM\_ReTx\_Mcast\_HARQ\_Disb] | 4504 | - | Release 17 |  |
| RP-23xxxxx: UE capability for Enhanced channel raster | XXXX | X | Release 16 |  |

<End of changes>