**3GPP TSG-RAN2 Meeting #125 *draft-*R2-2401987**

**Athens, Greece, 26th Feb – 1st Mar, 2024**

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  | **38.331** | **CR** | **4572** | **rev** | **2** | **Current version:** | **18.0.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network | **X** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Introduction of 2Rx XR UE [2Rx\_XR\_Device] |
|  |  |
| ***Source to WG:*** | Apple Inc., Vodafone, AT&T |
| ***Source to TSG:*** | R2 |
|  |  |
| ***Work item code:*** | NR\_TEI18, NR\_XR\_enh-Core |  | ***Date:*** | 2024-03-07 |
|  |  |  |  |  |
| ***Category:*** | **B** |  | ***Release:*** | Rel-18 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)**Rel-19 (Release 19)* |
|  |   |
| ***Reason for change:*** | Introduce 2Rx XR UEs to Rel-18. |
|  |  |
| ***Summary of change:*** | The following changes are added:1. clause 3.1: Add definiton of 2Rx XR UE;
2. clause 5.2.2.4.1: Add 2Rx XR UE to the types of Ues which shall acquire SIB1 if cellBarred is set in MIB;
3. clause 5.2.2.4.2: Add UE behavior for 2Rx XR Ues after acquiring SIB1, specifically how to respond to cell barring and intra-freq reselection indications specific to 2Rx XR Ues;
4. clause 5.2.2.4.5: Add UE behavior for 2Rx XR Ues after acquiring SIB4, specifically how to respond to inter-freq carrier information specific to 2Rx XR Ues;
5. clause 5.2.2.5: Add UE behavior for 2Rx XR Ues if MIB or SIB1 is missing;
6. clause 6.2.2, add cell barring and IFRI specific to 2Rx XR Ues to SIB1;
7. In SIB4, add new neighbouring frequency-specific cell re-selection information for 2Rx XR Ues;
8. clause 6.3.3: Add UE capability indication for support of 2Rx XR Ues.
9. Clause 11.2.2: Add a new indication to inter-node RRC message, *UERadioPagingInformation*, that the UE is a 2Rx XR UE.
 |
|  |  |
| ***Consequences if not approved:*** | 2Rx XR Ues can’t be supported in Rel-18. |
|  |  |
| ***Clauses affected:*** | 3.1, 5.2.2.4.1, 5.2.2.4.2, 5.2.2.4.5, 5.2.2.5, 6.3.1, 6.3.2, 6.3.3, 11.2.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** | **x** |  |  Other core specifications  | TS/TR 38.306.. CR 1052 |
| ***affected:*** |  | **x** |  Test specifications | TS/TR 38.304.. CR 0382 |
| ***(show related CRs)*** |  | **x** |  O&M Specifications | TS/TR 38.300.. CR 0813  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |
|  |  |

|  |
| --- |
| Start of the 1st change |

# 3 Definitions, symbols and abbreviations

## 3.1 Definitions

For the purposes of the present document, the terms and definitions given in TR 21.905 [1] and the following apply. A term defined in the present document takes precedence over the definition of the same term, if any, in TR 21.905 [1].

**2Rx XR UE:** two antenna port XR UE as specified in TS 38.101-1 [15].

**A2X communication:** A communication to support A2X services leveraging PC5 reference points, as defined in TS 23.256 [76]. A2X services are realized by various types of A2X applications, e.g., BRID or DAA.

**Aerial UE:** UE performingAerial UE communication, as defined in TS 38.300 [2], clause 16.18 and TS 23.256 [76].

**AM MRB:** An MRB associated with at least an AM RLC bearer for PTP transmission.

**BH RLC channel:** An RLC channel between two nodes, which is used to transport backhaul packets.

**Broadcast MRB:** A radio bearer configured for MBS broadcast delivery.

**CEIL:** Mathematical function used to 'round up' i.e. to the nearest integer having a higher or equal value.

**DAPS bearer:** a bearer whose radio protocols are located in both the source gNB and the target gNB during DAPS handover to use both source gNB and target gNB resources.

**Data Burst:** A set of multiple PDUs generated and sent by the application in a short period of time, as defined in TS 23.501 [32].

**Dedicated signalling:** Signalling sent on DCCH logical channel between the network and a single UE.

**Dormant BWP:** The dormant BWP is one of downlink BWPs configured by the network via dedicated RRC signalling. In the dormant BWP, the UE stops monitoring PDCCH on/for the SCell, but continues performing CSI measurements, Automatic Gain Control (AGC) and beam management, if configured. For each serving cell other than the SpCell or PUCCH SCell, the network may configure one BWP as a dormant BWP.

**eRedCap UE:** A UE with enhanced reduced capabilities as specified in clause 4.2.22.1 in TS 38.306 [26].

**Field:** The individual contents of an information element are referred to as fields.

**FLOOR:** Mathematical function used to 'round down' i.e. to the nearest integer having a lower or equal value.

**Frequency Selection Area ID:** An identity used for broadcast MBS session to guide the frequency selection of the UE as defined in TS 23.247 [67].

**Global cell identity:** An identity to uniquely identifying an NR cell. It is consisted of *cellIdentity* and *plmn-Identity* of the first *PLMN-Identity* in *plmn-IdentityList* in SIB1.

**Information element:** A structural element containing single or multiple fields is referred as information element.

**Candidate configuration:** A configuration part of an *RRCReconfiguration* message associated with a candidate cell, e.g., for LTM or subsequent CPAC. A candidate configuration can be a complete candidate configuration or a delta configuration relatively to a reference configuration.

**Reference configuration:** A configuration provided by the network to the UE that is common, within the same cell group, to a group of configured non-complete candidate configurations.

**MBS Radio Bearer:** A radio bearer that is configured for MBS delivery.

**Mobile IAB-MT**: mobile IAB-node function that terminates the Uu interface to the parent node using the procedures and behaviours specified for UEs unless stated otherwise.

**Mobile IAB-node**: RAN node that supports NR access links to UEs and an NR backhaul link to a parent node, and that can conduct physical mobility across the RAN area. The mobile IAB-node function used in 38-series of 3GPP Specifications corresponds to the MBSR function defined in TS 23.501 [32].

**Multicast/Broadcast Service:** A point-to-multipoint service as defined in TS 23.247 [67].

**Multicast MRB:** A radio bearer configured for MBS multicast delivery.

**MUSIM gap:** Period that the UE may use to perform MUSIM operations.

**Multi-path:** Mode of operation of a UE in RRC\_CONNECTED configured with one direct path on which the UE connects to gNB using NR Uu, and one indirect path on which the UE connects to the same gNB via another UE using PC5 unicast link or Non-3GPP Connection.

**MP remote UE:** A UE configured with Multi-path. When the connectivity of indirect path is PC5 unicast link, the MP remote UE is acting as a L2 U2N Remote UE. When the connectivity of indirect path is Non-3GPP Connection, the MP remote UE is acting as a N3C remote UE.

**MP relay UE:** A UE that provides connectivity of indirect path to a MP remote UE. When the connectivity is PC5 unicast link, the MP relay UE is acting as a L2 U2N Relay UE. When the connectivity is Non-3GPP Connection, the MP relay UE is acting as a N3C relay UE.

**NCSG:** Network controlled small gap as defined in TS 38.133 [14].

**NPN-only Cell**: A cell that is only available for normal service for NPNs' subscriber. An NPN-capable UE determines that a cell is NPN-only Cell by detecting that the *cellReservedForOtherUse* IE is set to true while the *npn-IdentityInfoList* IE is present in *CellAccessRelatedInfo*.

**N3C indirect path:** In Multi-path, the indirect path using Non-3GPP Connection between remote UE and relay UE.

**NR sidelink communication**: AS functionality enabling at least V2X Communication as defined in TS 23.287 [55], and ProSe Communication (including ProSe UE-to-Network Relay, non-Relay communication and ProSe UE-to-UE Relay Communication) as defined in TS 23.304 [65] between two or more nearby UEs, using NR technology but not traversing any network node.

**NR sidelink discovery**: AS functionality enabling ProSe non-Relay Discovery, ProSe UE-to-Network Relay discovery and ProSe UE-to-UE Relay discovery for Proximity based Services as defined in TS 23.304 [65] between two or more nearby UEs, using NR technology but not traversing any network node.

**NR sidelink positioning:** AS functionality enabling absolute positioning of a target UE or ranging via PC5 interface using SL-PRS transmission and reception as defined in TS 38.305 [73] and TS 38.355 [77].

**PNI-NPN identity:** an identifier of a PNI-NPN comprising of a PLMN ID and a CAG-ID combination.

**Primary Cell**: The MCG cell, operating on the primary frequency, in which the UE either performs the initial connection establishment procedure or initiates the connection re-establishment procedure.

**PC5 Relay RLC channel**: An RLC channel between L2 U2N Remote UE and L2 U2N Relay UE, or between L2 U2U Remote UE and L2 U2U Relay UE, which is used to transport packets over PC5 for L2 UE-to-Network relay or L2 UE-to-UE relay.

**Primary SCG Cell**: For dual connectivity operation, the SCG cell in which the UE performs random access when performing the Reconfiguration with Sync procedure.

**Primary Timing Advance Group**: Timing Advance Group containing the SpCell.

**PUCCH SCell:** An SCell configured with PUCCH by *PUCCH-Config*.

**PUSCH-Less SCell:** An SCell configured without PUSCH.

**RedCap UE:** A UE with reduced capabilities as specified in clause 4.2.21.1 in TS 38.306 [26].

**RLC bearer configuration:** The lower layer part of the radio bearer configuration comprising the RLC and logical channel configurations.

**Secondary Cell**: For a UE configured with CA, a cell providing additional radio resources on top of Special Cell.

**Secondary Cell Group**: For a UE configured with dual connectivity, the subset of serving cells comprising of the PSCell and zero or more secondary cells.

**Serving Cell**: For a UE in RRC\_CONNECTED not configured with CA/DC there is only one serving cell comprising of the primary cell. For a UE in RRC\_CONNECTED configured with CA/ DC the term 'serving cells' is used to denote the set of cells comprising of the Special Cell(s) and all secondary cells.

**Small Data Transmission**: A procedure used for transmission of data and/or signalling over allowed radio bearers in RRC\_INACTIVE state (i.e. without the UE transitioning to RRC\_CONNECTED state).

**SNPN identity:** an identifier of an SNPN comprising of a PLMN ID and an NID combination.

**SL indirect path:** In Multi-path, the indirect path using PC5 unicast link between remote UE and relay UE.

**Special Cell:** For Dual Connectivity operation the term Special Cell refers to the PCell of the MCG or the PSCell of the SCG, otherwise the term Special Cell refers to the PCell.

**Split DRB:** In MR-DC or MP, a DRB that supports transmission via MCG and SCG/indirect path in MP, as well as duplication of PDCP PDUs as defined in TS 37.340 [41].

**Split SRB**: In MR-DC or MP, an SRB that supports transmission via MCG and SCG/indirect path in MP as well as duplication of RRC PDUs as defined in TS 37.340 [41].

**SSB Frequency**: Frequency referring to the position of resource element RE=#0 (subcarrier #0) of resource block RB#10 of the SS block.

**U2N Relay UE**: A UE that provides functionality to support connectivity to the network for U2N Remote UE(s).

**U2N Remote UE**: A UE that communicates with the network via a U2N Relay UE.

**U2U Relay UE:** A UE that provides functionality to support connectivity between U2U Remote UEs.

**U2U Remote UE:** A UE that communicates with another UE via a U2U Relay UE.

**Uu Relay RLC channel**: An RLC channel between L2 U2N Relay UE and gNB, which is used to transport packets over Uu for L2 UE-to-Network relay or for indirect path in case of MP**.**

**UE Inactive AS Context**: UE Inactive AS Context is stored when the connection is suspended and restored when the connection is resumed. It includes information as defined in clause 5.3.8.3.

**V2X sidelink communication**: AS functionality enabling V2X Communication as defined in TS 23.285 [56], between nearby UEs, using E-UTRA technology but not traversing any network node.

|  |
| --- |
| End of the 1st change |

|  |
| --- |
| Start of the 2nd change |

## 5.2 System information

##### 5.2.2.4.1 Actions upon reception of the *MIB*

Upon receiving the *MIB* the UE shall:

1> store the acquired *MIB*;

1> if the UE is in RRC\_IDLE or in RRC\_INACTIVE, or if the UE is in RRC\_CONNECTED while *T311* is running:

2> if the access is not for NTN or the UE is not capable of NTN or the UE is not capable of NES cell DTX/DRX; and

2> if the access is not for ATG or the UE is not capable of ATG; and

2> if the *cellBarred* in the acquired *MIB* is set to *barred*:

3> if the UE is an (e)RedCap UE or a 2Rx XR UE and if *ssb-SubcarrierOffset* indicates *SIB1* is transmitted in the cell (TS 38.213 [13]):

4> acquire the *SIB1,* which is scheduled as specified in TS 38.213 [13];

3> consider the cell as barred in accordance with TS 38.304 [20];

3> perform cell re-selection to other cells on the same frequency as the barred cell as specified in TS 38.304 [20];

2> else:

3> apply the received *systemFrameNumber*, *pdcch-ConfigSIB1*, *subCarrierSpacingCommon*, *ssb-SubcarrierOffset* and *dmrs-TypeA-Position*.

NOTE 1: A UE capable of NTN access should acquire SIB1 to determine whether the cell is an NTN cell.

NOTE 2: A UE capable of ATG access should acquire SIB1 to determine whether the cell is an ATG cell.

NOTE 3: A UE capable of NES cell DTX/DRX should acquire SIB1 to determine the cell barring status when the *cellBarred* in MIB is set to *barred*.

|  |
| --- |
| End of the 2nd change |

|  |
| --- |
| Start of the 3rd change |

#### 5.2.2.4 Actions upon receipt of System Information

##### 5.2.2.4.2 Actions upon reception of the *SIB1*

Upon receiving the *SIB1* the UE shall:

1> store the acquired *SIB1*;

1> if the access is for NTN:

2> if the UE is in RRC\_IDLE or in RRC\_INACTIVE, or if the UE is in RRC\_CONNECTED while *T311* is running; and

2> if the *cellBarredNTN* in the acquired *SIB1* is set to *barred* or the *cellBarredNTN* is not included in the acquired *SIB1*:

3> consider the cell as barred in accordance with TS 38.304 [20];

3> perform cell re-selection to other cells on the same frequency as the barred cell as specified in TS 38.304 [20], upon which the procedure ends;

1> if the access is for ATG:

2> if the UE is in RRC\_IDLE or in RRC\_INACTIVE, or if the UE is in RRC\_CONNECTED while *T311* is running; and

2> if the *cellBarredNTN* in the acquired *SIB1* is set to *barred* or the *cellBarredNTN* is not included in the acquired *SIB1*:

3> consider the cell as barred in accordance with TS 38.304 [20];

3> perform cell re-selection to other cells on the same frequency as the barred cell as specified in TS 38.304 [20];

1> if the UE is a RedCap UE and it is in RRC\_IDLE or in RRC\_INACTIVE, or if the RedCap UE is in RRC\_CONNECTED while *T311* is running:

2> if *intraFreqReselectionRedCap* is not present in *SIB1*:

3> consider the cell as barred in accordance with TS 38.304 [20];

3> perform barring as if *intraFreqReselectionRedCap* is set to allowed, upon which the procedure ends;

2> else:

3> if the *cellBarredRedCap1Rx* is present in the acquired *SIB1* and is set to *barred* and the UE is equipped with 1 Rx branch; or

3> if the *cellBarredRedCap2Rx* is present in the acquired *SIB1* and is set to *barred* and the UE is equipped with 2 Rx branches; or

3> if the *halfDuplexRedCapAllowed* is not present in the acquired *SIB1* and the UE supports only half-duplex FDD operation:

4> consider the cell as barred in accordance with TS 38.304 [20];

4> perform barring based on *intraFreqReselectionRedCap* as specified in TS 38.304 [20], upon which the procedure ends;

1> if the UE is a 2Rx XR UE and is in RRC\_IDLE or in RRC\_INACTIVE, or if the 2Rx XR UE is in RRC\_CONNECTED while *T311* is running:

2> if the *cellBarred2RxXR* is present in the acquired *SIB1*:

3> consider the cell as barred in accordance with TS 38.304 [20];

4> if the *intraFreqReselection2RxXR* is present in the acquired *SIB1*;

4> perform barring based on *intraFreqReselection2RxXR* as specified in TS 38.304 [20] upon which the procedure ends;

4> else:

5> perform barring as if *intraFreqReselection2RxXR* is set to allowed upon which the procedure ends;1> if the UE supports NES cell DTX/DRX and it is in RRC\_IDLE or in RRC\_INACTIVE, or if the UE supporting NES cell DTX/DRX is in RRC\_CONNECTED while *T311* is running:

2> if *cellBarred* in the acquired *MIB* is set to *barred*:

3> if *cellBarredNES* is absent in the acquired *SIB1:*

4> consider the cell as barred in accordance with TS 38.304 [20];

4> perform cell re-selection to other cells on the same frequency as the barred cell as specified in TS 38.304 [20];

1> if the UE is an eRedCap UE and it is in RRC\_IDLE or in RRC\_INACTIVE, or if the eRedCap UE is in RRC\_CONNECTED while *T311* is running:

2> if *intraFreqReselection-eRedCap* is not present in *SIB1*:

3> consider the cell as barred in accordance with TS 38.304 [20];

3> perform barring as if *intraFreqReselection-eRedCap* is set to allowed upon which the procedure ends;

2> else:

3> if the *cellBarred-eRedCap1Rx* is present in the acquired *SIB1* and is set to *barred* and the UE is equipped with 1 Rx branch; or

3> if the *cellBarred-eRedCap2Rx* is present in the acquired *SIB1* and is set to *barred* and the UE is equipped with 2 Rx branches; or

3> if the *halfDuplexRedCapAllowed* is not present in the acquired *SIB1* and the UE supports only half-duplex FDD operation:

4> consider the cell as barred in accordance with TS 38.304 [20];

4> perform barring based on *intraFreqReselection-eRedCap* as specified in TS 38.304 [20] upon which the procedure ends;

1> if the *cellAccessRelatedInfo* contains an entry of a selected SNPN or PLMN and in case of PLMN the UE is either allowed or instructed to access the PLMN via a cell for which at least one CAG ID is broadcast:

2> in the remainder of the procedures use *npn-IdentityList, trackingAreaCode,* and *cellIdentity* for the cell as received in the corresponding entry of *npn-IdentityInfoList* containing the selected PLMN or SNPN;

1> else if the *cellAccessRelatedInfo* contains an entry with the *PLMN-Identity* of the selected PLMN:

2> in the remainder of the procedures use *plmn-IdentityList*, *trackingAreaCode*, *trackingAreaList,* and *cellIdentity* for the cell as received in the corresponding *PLMN-IdentityInfo* containing the selected PLMN;

1> if the UE in RRC\_INACTIVE is configured for feature(s) that it does not support in current serving cell:

2> not use the corresponding configuration in current serving cell;

NOTE 0: The requirement above applies only to UE that indicates different support of UE capabilities for TN and NTN.

1> if in RRC\_CONNECTED while T311 is not running:

2> disregard the *frequencyBandList*, if received, while in RRC\_CONNECTED;

2> forward the *cellIdentity* to upper layers;

2> forward the *trackingAreaCode* to upper layers, if included;

2> forward the *trackingAreaList* to upper layers, if included;

2> forward the received *posSIB-MappingInfo* to upper layers, if included;

2> apply the configuration included in the *servingCellConfigCommon*;

2> if the UE has a stored valid version of a SIB or posSIB, in accordance with clause 5.2.2.2.1, that the UE requires to operate within the cell in accordance with clause 5.2.2.1:

3> use the stored version of the required SIB or posSIB;

2> else:

3> acquire the required SIB or posSIB requested by upper layer as defined in clause 5.2.2.3.5;

NOTE 1: Void.

1> else:

2> if the UE supports one or more of the frequency bands indicated in the *frequencyBandList or frequencyBandListAerial* for downlink for TDD, or one or more of the frequency bands indicated in the *frequencyBandList* or *frequencyBandListAerial* for uplink for FDD, and they are not downlink only bands, and

2> if the UE is IAB-MT or supports at least one *additionalSpectrumEmission* in the *nr-NS-PmaxList* or *nr-NS-PmaxListAerial* for a supported band in the downlink for TDD, or a supported band in uplink for FDD, and

2> if the UE supports an uplink channel bandwidth with a maximum transmission bandwidth configuration (see TS 38.101-1 [15], TS 38.101-2 [39], and TS 38.101-5 [75]) which

- is smaller than or equal to the *carrierBandwidth* (indicated in *uplinkConfigCommon* for the SCS of the initial uplink BWP or, for (e)RedCap UE, of the (e)RedCap-specific initial uplink BWP if configured), and which

- is wider than or equal to the bandwidth of the initial uplink BWP or, for (e)RedCap UE, of the (e)RedCap-specific initial uplink BWP if configured, and

2> if the UE supports a downlink channel bandwidth with a maximum transmission bandwidth configuration (see TS 38.101-1 [15], TS 38.101-2 [39], and TS 38.101-5 [75]) which

- is smaller than or equal to the *carrierBandwidth* (indicated in *downlinkConfigCommon* for the SCS of the initial downlink BWP or, for (e)RedCap UE, of the (e)RedCap-specific initial downlink BWP if configured), and which

- is wider than or equal to the bandwidth of the initial downlink BWP or, for (e)RedCap UE, of the (e)RedCap-specific initial downlink BWP if configured, and

2> if *frequencyShift7p5khz* is present and the UE supports corresponding 7.5kHz frequency shift on this band; or *frequencyShift7p5khz* is not present, and

2> if the UE is not a RedCap UE, or if the UE is a RedCap UE and *halfDuplexRedCapAllowed* is present, or if the UE is a RedCap UE and the RedCap UE supports full-duplex FDD operation on this band:

3> if neither *trackingAreaCode* nor *trackingAreaList* is provided for the selected PLMN nor the registered PLMN nor PLMN of the equivalent PLMN list:

4> consider the cell as barred in accordance with TS 38.304 [20];

4> perform cell re-selection to other cells on the same frequency as the barred cell as specified in TS 38.304 [20];

3> else if UE is IAB-MT and if *iab-Support* is not provided for the selected PLMN nor the registered PLMN nor PLMN of the equivalent PLMN list nor the selected SNPN nor the registered SNPN nor SNPN of the equivalent SNPN list:

4> consider the cell as barred in accordance with TS 38.304 [20];

3> else if UE is NCR-MT and if *ncr-Support* is not provided:

4> consider the cell as barred in accordance with TS 38.304 [20];

3> else if UE is a mobile IAB-MT and if *mobileIAB-Support* is not provided for the selected PLMN nor the registered PLMN nor PLMN of the equivalent PLMN list nor the selected SNPN nor the registered SNPN nor SNPN of the equivalent SNPN list:

4> consider the cell as barred in accordance with TS 38.304 [20];

*Editor's Note: FFS whether a cell can be barred for a mobile IAB-MT.*

3> else:

4> apply a supported uplink channel bandwidth with a maximum transmission bandwidth which

- is contained within the *carrierBandwidth* indicated in *uplinkConfigCommon* for the SCS of the initial uplink BWP or, for (e)RedCap UEs, (e)RedCap-specific initial uplink BWP, if configured, and which

- is wider than or equal to the bandwidth of the initial BWP for the uplink or, for a (e)RedCap UE, of the (e)RedCap-specific initial uplink BWP if configured;

4> apply a supported downlink channel bandwidth with a maximum transmission bandwidth which

- is contained within the *carrierBandwidth* indicated in *downlinkConfigCommon* for the SCS of the initial downlink BWP or, for (e)RedCap UEs, (e)RedCap-specific initial downlink BWP, if configured, and which

- is wider than or equal to the bandwidth of the initial BWP for the downlink or, for a (e)RedCap UE, of the (e)RedCap-specific initial downlink BWP if configured;

4> if the UE is aerial UE and it supports at least one frequency band in the *frequencyBandListAerial*, for FDD from *frequencyBandListAerial* for uplink, or for TDD from *frequencyBandListAerial* for downlink,for which the UE supports at least one of the *additionalSpectrumEmission* values in *nr-NS-PmaxListAerial*, if present:

5> select the first frequency band in the *frequencyBandListAerial*, for FDD from *frequencyBandListAerial* for uplink, or for TDD from *frequencyBandListAerial* for downlink,which the UE supports and for which the UE supports at least one of the *additionalSpectrumEmission* values in *nr-NS-PmaxListAerial*;

4> else:

5> select the first frequency band in the *frequencyBandList*, for FDD from *frequencyBandList* for uplink, or for TDD from *frequencyBandList* for downlink,which the UE supports and for which the UE supports at least one of the *additionalSpectrumEmission* values in *nr-NS-PmaxList*, if present, and for RedCap UEs if the *halfDuplexRedCapAllowed* is not present, for which the UE supports full-duplex FDD operation;

4> forward the *cellIdentity* to upper layers;

4> forward the *trackingAreaCode* to upper layers;

4> forward the *trackingAreaList* to upper layers, if included;

4> forward the received *posSIB-MappingInfo* to upper layers, if included;

4> forward the PLMN identity or SNPN identity or PNI-NPN identity to upper layers;

4> if in RRC\_INACTIVE and the forwarded information does not trigger message transmission by upper layers:

5> if the serving cell does not belong to the configured *ran-NotificationAreaInfo*:

6> initiate an RNA update as specified in 5.3.13.8;

5> if configured to receive MBS multicast in RRC\_INACTIVE and not indicated to stop monitoring G-RNTI for at least one MBS multicast session:

6> if SIB24 is not scheduled in SIB1 in the cell after cell selection or cell reselection:

7> initiate an RRC connection resume procedure for multicast reception as specified in 5.3.13.1d;

4> forward the *ims-EmergencySupport* to upper layers, if present;

4> forward the *eCallOverIMS-Support* to upper layers, if present;

4> forward the *UAC-AccessCategory1-SelectionAssistanceInfo* or *UAC-AC1-SelectAssistInfo* for the selected PLMN/SNPNto upper layers, if present and set to *a*, *b* or *c*;

4> if the UE is in SNPN access mode:

5> forward the *imsEmergencySupportForSNPN* indicators with the corresponding SNPN identities to upper layers, if present;

4> apply the configuration included in the *servingCellConfigCommon*;

4> apply the specified PCCH configuration defined in 9.1.1.3;

4> if the UE has a stored valid version of a SIB, in accordance with clause 5.2.2.2.1, that the UE requires to operate within the cell in accordance with clause 5.2.2.1:

5> use the stored version of the required SIB;

4> if the UE has not stored a valid version of a SIB, in accordance with clause 5.2.2.2.1, of one or several required SIB(s), in accordance with clause 5.2.2.1:

5> for the SI message(s) that, according to the *si-SchedulingInfo*, contain at least one required SIB and for which *si-BroadcastStatus* is set to broadcasting:

6> acquire the SI message(s) as defined in clause 5.2.2.3.2;

5> for the SI message(s) that, according to the *si-SchedulingInfo*, contain at least one required SIB and for which *si-BroadcastStatus* is set to *notBroadcasting*:

6> trigger a request to acquire the SI message(s) as defined in clause 5.2.2.3.3;

4> if the UE has a stored valid version of a posSIB, in accordance with clause 5.2.2.2.1, of one or several required posSIB(s), in accordance with clause 5.2.2.1:

5> use the stored version of the required posSIB;

4> if the UE has not stored a valid version of a posSIB, in accordance with clause 5.2.2.2.1, of one or several posSIB(s) in accordance with clause 5.2.2.1:

5> for the SI message(s) that, according to the *posSI-SchedulingInfo*, contain at least one requested posSIB and for which *posSI-BroadcastStatus* is set to *broadcasting*:

6> acquire the SI message(s) as defined in clause 5.2.2.3.2;

5> for the SI message(s) that, according to the *posSI-SchedulingInfo*, contain at least one requested posSIB for which *posSI-BroadcastStatus* is set to *notBroadcasting*:

6> trigger a request to acquire the SI message(s) as defined in clause 5.2.2.3.3a;

4> if the UE is aerial UE and it supports at least one *additionalSpectrumEmission* values in *nr-NS-PmaxListAerial* within *frequencyBandListAerial* in *uplinkConfigCommon* for FDD or in *downlinkConfigCommon* for TDD:

5> apply the first listed *additionalSpectrumEmission* which it supports among the values included in *nr-NS-PmaxListAerial* within *frequencyBandListAerial* in *uplinkConfigCommon* for FDD or in *downlinkConfigCommon* for TDD;

4> else:

5> apply the first listed *additionalSpectrumEmission* which it supports among the values included in *nr-NS-PmaxList* within *frequencyBandList* in *uplinkConfigCommon* for FDD or in *downlinkConfigCommon* for TDD;

4> if the *additionalPmax* is present in the same entry of the selected *additionalSpectrumEmission* within *nr-NS-PmaxList* or *nr-NS-PmaxListAerial*:

5> apply the *additionalPmax* for UL;

4> else:

5> apply the *p-Max* in *uplinkConfigCommon* for UL;

4> if *supplementaryUplink* is present in *servingCellConfigCommon*; and

4> if the UE supports one or more of the frequency bands indicated in the *frequencyBandList* for the *supplementaryUplink*; and

4> if the UE supports at least one *additionalSpectrumEmission* in the *nr-NS-PmaxList* for a supported supplementary uplink band; and

4> if the UE is not a RedCap UE, or if the UE is a RedCap UE and *halfDuplexRedCapAllowed* is present, or if the UE is a RedCap UE and the RedCap UE supports full-duplex FDD operation on the frequency bands indicated in the *frequencyBandList* for the *supplementaryUplink*; and

4> if the UE supports an uplink channel bandwidth with a maximum transmission bandwidth configuration (see TS 38.101-1 [15] and TS 38.101-2 [39]) which

- is smaller than or equal to the *carrierBandwidth* (indicated in *supplementaryUplink* for the SCS of the initial uplink BWP), and which

- is wider than or equal to the bandwidth of the initial uplink BWP of the SUL:

5> consider supplementary uplink as configured in the serving cell;

5> select the first frequency band in the *frequencyBandList* for the *supplementaryUplink* which the UE supports and for which the UE supports at least one of the *additionalSpectrumEmission* values in *nr-NS-PmaxList*, if present, and for RedCap UEs if the *halfDuplexRedCapAllowed* is not present, for which the UE supports full-duplex FDD operation;

5> apply a supported supplementary uplink channel bandwidth with a maximum transmission bandwidth which

- is contained within the *carrierBandwidth* (indicated in *supplementaryUplink* for the SCS of the initial uplink BWP), and which

- is wider than or equal to the bandwidth of the initial BWP of the SUL;

5> apply the first listed *additionalSpectrumEmission* which it supports among the values included in *nr-NS-PmaxList* within *frequencyBandList* for the *supplementaryUplink*;

5> if the *additionalPmax* is present in the same entry of the selected *additionalSpectrumEmission* within *nr-NS-PmaxList* for the *supplementaryUplink*:

6> apply the *additionalPmax* in *supplementaryUplink* for SUL;

5> else:

6> apply the *p-Max* in *supplementaryUplink* for SUL;

NOTE 2: For an out of coverage L2 U2N Remote UE in RRC\_IDLE or RRC\_INACTIVE receiving SIB1 from its connected L2 U2N Relay UE, it is up to Remote UE implementation whether to consider and apply the following parameters: *frequencyBandList*, *carrierBandwidth*, *frequencyShift7p5khz*, frequency band, channel bandwidth, the configuration included in the *servingCellConfigCommon*, the specified PCCH configuration, *additionalSpectrumEmission*, *additionalPmax*, and *p-Max*.

2> else:

3> consider the cell as barred in accordance with TS 38.304 [20]; and

3> perform barring as if *intraFreqReselection*, or *intraFreqReselectionRedCap* for RedCap UEs, or *intraFreqReselection-eRedCap* for eRedCap UEs, or *intraFreqReselection2RxXR* for 2Rx XR UEs is set to *notAllowed*;

##### 5.2.2.4.5 Actions upon reception of *SIB4*

Upon receiving *SIB4* the UE shall:

1> if in RRC\_IDLE, or in RRC\_INACTIVE or in RRC\_CONNECTED while T311 is running:

2> for each entry in the *interFreqCarrierFreqList*:

3> if the UE is neither a RedCap nor an eRedCap UE nor 2Rx XR UE; or

3> if the UE is a RedCap UE and the *interFreqCarrierFreqList-v1700* is absent; or

3> if the UE is an eRedCap UE and the *interFreqCarrierFreqList-v1800* is absent; or

3> if the UE is a 2Rx XR UE and the *interFreqCarrierFreqList-v1800* is absent; or

3> if the UE is a RedCap UE and *redCapAccessAllowed* is present in *interFreqCarrierFreqList-v1700;* or

3> if the UE is an eRedCap UE and e*RedCapAccessAllowed* is present in *interFreqCarrierFreqList-v1800; or*

3> if the UE is a 2Rx XR UE and *AccessAllowed2RxXR* is present in *interFreqCarrierFreqList-v1800*:

4> select the first frequency band in the *frequencyBandList* (or for aerial UE *frequencyBandListAerial*), and *frequencyBandListSUL*, if present, which the UE supports and for which the UE supports at least one of the *additionalSpectrumEmission* values in *nr-NS-PmaxList* (or for aerial UE *nr-NS-PmaxListAerial*), if present:

4> if, the frequency band selected by the UE in *frequencyBandList* or *frequencyBandListAerial* to represent a non-serving NR carrier frequency is not a downlink only band:

5> if, for the selected frequency band, the UE supports at least one *additionalSpectrumEmission* in the *nr-NS-PmaxList* within the *frequencyBandList*; or

5> if, for the selected frequency band, the UE supports at least one *additionalSpectrumEmission* in the *nr-NS-PmaxListAerial* within the *frequencyBandListAerial*:

6> if the UE is aerial UE and it supports at least one *additionalSpectrumEmission* values in *nr-NS-PmaxListAerial* within the *frequencyBandListAerial*:

7> apply the first listed *additionalSpectrumEmission* which it supports among the values included in *nr-NS-PmaxListAerial* within *frequencyBandListAerial*;

6> else:

7> apply the first listed *additionalSpectrumEmission* which it supports among the values included in *nr-NS-PmaxList* within *frequencyBandList*;

6> if the *additionalPmax* is present in the same entry of the selected *additionalSpectrumEmission* within *nr-NS-PmaxList* or *nr-NS-PmaxListAerial*:

7> apply the *additionalPmax*;

6> else:

7> apply the *p-Max*;

6> if frequencyBandListSUL is present in SIB4 and, for the frequency band selected in frequencyBandListSUL, the UE supports at least one *additionalSpectrumEmission* in the *nr-NS-PmaxList* within *FrequencyBandListSUL*:

7> apply the first listed *additionalSpectrumEmission* which it supports among the values included in *nr-NS-PmaxList* within *frequencyBandListSUL*;

7> if the *additionalPmax* is present in the same entry of the selected *additionalSpectrumEmission* within *nr-NS-PmaxList*:

8> apply the *additionalPmax*;

7> else:

8> apply the *p-Max*;

6> else:

7> apply the *p-Max*;

5> else:

6> apply the *p-Max*;

1> if in RRC\_IDLE or RRC\_INACTIVE, and T331 is running:

2> perform the actions as specified in 5.7.8.1a;

<<next change>>

#### 5.2.2.5 Essential system information missing

The UE shall:

1> if in RRC\_IDLE or in RRC\_INACTIVE or in RRC\_CONNECTED while T311 is running:

2> if the UE is unable to acquire the *MIB*:

3> consider the cell as barred in accordance with TS 38.304 [20];

3> perform barring as if *intraFreqReselection*, or *intraFreqReselectionRedCap* for RedCap UEs, or *intraFreqReselection-eRedCap* for eRedCap UEs or *intraFreqReselection2RxXR* for 2Rx XR UEs is set to *allowed*;

2> else if the UE is unable to acquire the *SIB1*:

3> consider the cell as barred in accordance with TS 38.304 [20];

3> if the UE is a RedCap UE:

4> perform barring as if *intraFreqReselectionRedCap* is set to *allowed*;

3> else if the UE is an eRedCap UE:

4> perform barring as if *intraFreqReselection-eRedCap* is set to *allowed*;

3> else if the UE is a 2Rx XR UE:

4> perform barring as if *intraFreqReselection2RxXR* is set to *allowed*;

3> else:

4> perform cell re-selection to other cells on the same frequency as the barred cell as specified in TS 38.304 [20].

NOTE 1: The *SIB19* is essential for NTN access. If UE is unable to acquire the *SIB19* for NTN access, the action is up to UE implementation (e.g., cell re-selection to other cells).

NOTE 2: The *SIB22* is essential for ATG access. If UE is unable to acquire the *SIB22* for ATG access, the action is up to UE implementation (e.g., cell re-selection to other cells).

# 6 Protocol data units, formats and parameters (ASN.1)

### 6.2.2 Message definitions

#### – *SIB1*

*SIB1* contains information relevant when evaluating if a UE is allowed to access a cell and defines the scheduling of other system information.It also contains radio resource configuration information that is common for all UEs and barring information applied to the unified access control.

Signalling radio bearer: N/A

RLC-SAP: TM

Logical channels: BCCH

Direction: Network to UE

*SIB1* message

-- ASN1START

-- TAG-SIB1-START

SIB1 ::= SEQUENCE {

 cellSelectionInfo SEQUENCE {

 q-RxLevMin Q-RxLevMin,

 q-RxLevMinOffset INTEGER (1..8) OPTIONAL, -- Need S

 q-RxLevMinSUL Q-RxLevMin OPTIONAL, -- Need R

 q-QualMin Q-QualMin OPTIONAL, -- Need S

 q-QualMinOffset INTEGER (1..8) OPTIONAL -- Need S

 } OPTIONAL, -- Cond Standalone

 cellAccessRelatedInfo CellAccessRelatedInfo,

 connEstFailureControl ConnEstFailureControl OPTIONAL, -- Need R

 si-SchedulingInfo SI-SchedulingInfo OPTIONAL, -- Need R

 servingCellConfigCommon ServingCellConfigCommonSIB OPTIONAL, -- Need R

 ims-EmergencySupport ENUMERATED {true} OPTIONAL, -- Need R

 eCallOverIMS-Support ENUMERATED {true} OPTIONAL, -- Need R

 ue-TimersAndConstants UE-TimersAndConstants OPTIONAL, -- Need R

 uac-BarringInfo SEQUENCE {

 uac-BarringForCommon UAC-BarringPerCatList OPTIONAL, -- Need S

 uac-BarringPerPLMN-List UAC-BarringPerPLMN-List OPTIONAL, -- Need S

 uac-BarringInfoSetList UAC-BarringInfoSetList,

 uac-AccessCategory1-SelectionAssistanceInfo CHOICE {

 plmnCommon UAC-AccessCategory1-SelectionAssistanceInfo,

 individualPLMNList SEQUENCE (SIZE (2..maxPLMN)) OF UAC-AccessCategory1-SelectionAssistanceInfo

 } OPTIONAL -- Need S

 } OPTIONAL, -- Need R

 useFullResumeID ENUMERATED {true} OPTIONAL, -- Need R

 lateNonCriticalExtension OCTET STRING OPTIONAL,

 nonCriticalExtension SIB1-v1610-IEs OPTIONAL

}

SIB1-v1610-IEs ::= SEQUENCE {

 idleModeMeasurementsEUTRA-r16 ENUMERATED{true} OPTIONAL, -- Need R

 idleModeMeasurementsNR-r16 ENUMERATED{true} OPTIONAL, -- Need R

 posSI-SchedulingInfo-r16 PosSI-SchedulingInfo-r16 OPTIONAL, -- Need R

 nonCriticalExtension SIB1-v1630-IEs OPTIONAL

}

SIB1-v1630-IEs ::= SEQUENCE {

 uac-BarringInfo-v1630 SEQUENCE {

 uac-AC1-SelectAssistInfo-r16 SEQUENCE (SIZE (2..maxPLMN)) OF UAC-AC1-SelectAssistInfo-r16

 } OPTIONAL, -- Need R

 nonCriticalExtension SIB1-v1700-IEs OPTIONAL

}

SIB1-v1700-IEs ::= SEQUENCE {

 hsdn-Cell-r17 ENUMERATED {true} OPTIONAL, -- Need R

 uac-BarringInfo-v1700 SEQUENCE {

 uac-BarringInfoSetList-v1700 UAC-BarringInfoSetList-v1700

 } OPTIONAL, -- Cond MINT

 sdt-ConfigCommon-r17 SDT-ConfigCommonSIB-r17 OPTIONAL, -- Need R

 redCap-ConfigCommon-r17 RedCap-ConfigCommonSIB-r17 OPTIONAL, -- Need R

 featurePriorities-r17 SEQUENCE {

 redCapPriority-r17 FeaturePriority-r17 OPTIONAL, -- Need R

 slicingPriority-r17 FeaturePriority-r17 OPTIONAL, -- Need R

 msg3-Repetitions-Priority-r17 FeaturePriority-r17 OPTIONAL, -- Need R

 sdt-Priority-r17 FeaturePriority-r17 OPTIONAL -- Need R

 } OPTIONAL, -- Need R

 si-SchedulingInfo-v1700 SI-SchedulingInfo-v1700 OPTIONAL, -- Need R

 hyperSFN-r17 BIT STRING (SIZE (10)) OPTIONAL, -- Need R

 eDRX-AllowedIdle-r17 ENUMERATED {true} OPTIONAL, -- Need R

 eDRX-AllowedInactive-r17 ENUMERATED {true} OPTIONAL, -- Cond EDRX-RC

 intraFreqReselectionRedCap-r17 ENUMERATED {allowed, notAllowed} OPTIONAL, -- Need S

 cellBarredNTN-r17 ENUMERATED {barred, notBarred} OPTIONAL, -- Need S

 nonCriticalExtension SIB1-v1740-IEs OPTIONAL

}

SIB1-v1740-IEs ::= SEQUENCE {

 si-SchedulingInfo-v1740 SI-SchedulingInfo-v1740 OPTIONAL, -- Need R

 nonCriticalExtension SIB1-v1800-IEs OPTIONAL

}

SIB1-v1800-IEs ::= SEQUENCE {

 ncr-Support-r18 ENUMERATED {true} OPTIONAL, -- Need S

 mt-SDT-ConfigCommonSIB-r18 MT-SDT-ConfigCommonSIB-r18 OPTIONAL, -- Need R

 musim-CapRestrictionAllowed-r18 ENUMERATED {true} OPTIONAL, -- Need R

 featurePriorities-v1800 SEQUENCE {

 msg1-Repetitions-Priority-r18 FeaturePriority-r17 OPTIONAL, -- Need R

 eRedCapPriority-r18 FeaturePriority-r17 OPTIONAL -- Need R

 } OPTIONAL, -- Need R

 si-SchedulingInfo-v1800 SI-SchedulingInfo-v1800 OPTIONAL, -- Need R

 cellBarredATG-r18 ENUMERATED {barred, notBarred} OPTIONAL, -- Need S

 cellBarredNES-r18 ENUMERATED {notBarred} OPTIONAL, -- Need R

 mobileIAB-Cell-r18 ENUMERATED {true} OPTIONAL, -- Need R

 eDRX-AllowedInactive-r18 ENUMERATED {true} OPTIONAL, -- Cond EDRX-RC

 intraFreqReselection-eRedCap-r18 ENUMERATED {allowed, notAllowed} OPTIONAL, -- Need S

 nonServingCellMII-r18 ENUMERATED {true} OPTIONAL, -- Need R

 cellBarred2RxXR-r18 ENUMERATED {true} OPTIONAL -- Need R

 intraFreqReselection2RxXR-r18 ENUMERATED {allowed, notAllowed} OPTIONAL -- Need R

 nonCriticalExtension SEQUENCE {} OPTIONAL

}

UAC-AccessCategory1-SelectionAssistanceInfo ::= ENUMERATED {a, b, c}

UAC-AC1-SelectAssistInfo-r16 ::= ENUMERATED {a, b, c, notConfigured}

SDT-ConfigCommonSIB-r17 ::= SEQUENCE {

 sdt-RSRP-Threshold-r17 RSRP-Range OPTIONAL, -- Need R

 sdt-LogicalChannelSR-DelayTimer-r17 ENUMERATED { sf20, sf40, sf64, sf128, sf512, sf1024, sf2560, spare1} OPTIONAL, -- Need R

 sdt-DataVolumeThreshold-r17 ENUMERATED {byte32, byte100, byte200, byte400, byte600, byte800, byte1000, byte2000, byte4000,

 byte8000, byte9000, byte10000, byte12000, byte24000, byte48000, byte96000},

 t319a-r17 ENUMERATED { ms100, ms200, ms300, ms400, ms600, ms1000, ms2000,

 ms3000, ms4000, spare7, spare6, spare5, spare4, spare3, spare2, spare1}

}

RedCap-ConfigCommonSIB-r17 ::= SEQUENCE {

 halfDuplexRedCapAllowed-r17 ENUMERATED {true} OPTIONAL, -- Need R

 cellBarredRedCap-r17 SEQUENCE {

 cellBarredRedCap1Rx-r17 ENUMERATED {barred, notBarred},

 cellBarredRedCap2Rx-r17 ENUMERATED {barred, notBarred}

 } OPTIONAL, -- Need R

 ...,

 [[

 cellBarredRedCap-r18 SEQUENCE {

 cellBarred-eRedCap1Rx-r18 ENUMERATED {barred, notBarred},

 cellBarred-eRedCap2Rx-r18 ENUMERATED {barred, notBarred}

 } OPTIONAL -- Need R

 ]]

}

FeaturePriority-r17 ::= INTEGER (0..7)

MT-SDT-ConfigCommonSIB-r18 ::= SEQUENCE {

 sdt-RSRP-ThresholdMT-r18 RSRP-Range OPTIONAL, -- Need S

 sdt-LogicalChannelSR-DelayTimer-r18 ENUMERATED { sf20, sf40, sf64, sf128, sf512, sf1024, sf2560, spare1} OPTIONAL, -- Cond MT-SDT1

 t319a-r18 ENUMERATED { ms100, ms200, ms300, ms400, ms600, ms1000, ms2000,

 ms3000, ms4000, spare7, spare6, spare5, spare4,

 spare3, spare2, spare1} OPTIONAL -- Cond MT-SDT2

}

-- TAG-SIB1-STOP

-- ASN1STOP

|  |
| --- |
| *SIB1* field descriptions |
| ***cellBarred2RxXR***Indicates whether the cell is barred for 2Rx XR UEs. This field is ignored by all UEs that are not 2Rx XR UEs. This field may be configured only if the cell operates in a frequency band where 4Rx antenna ports are mandated as specified in TS 38.101-1 [15]. If this field is absent on a cell operating in a frequency band where 4RX antenna ports are mandated, a 2RX XR UE shall treat the cell as not barred, as specified in TS 38.304 [20]. |
| ***cellBarredATG***Value *barred* means that the cell is barred for connectivity to ATG, as defined in TS 38.304 [20]. Value *notBarred* means that the cell is allowed for connectivity to ATG. If not present, the UE considers the cell is not allowed for connectivity to ATG, as defined in TS 38.304 [20]. This field is only applicable to ATG-capable UEs. |
| ***cellBarred-eRedCap1Rx***Value *barred* means that the cell is barred for an eRedCap UE with 1 Rx branch, as defined in TS 38.304 [20]. This field is ignored by non-eRedCap UEs. |
| ***cellBarred-eRedCap2Rx***Value *barred* means that the cell is barred for an eRedCap UE with 2 Rx branches, as defined in TS 38.304 [20]. This field is ignored by non-eRedCap UEs. |
| ***cellBarredNES***The presence of this field indicates that the cell is allowed for UEs supporting NES cell DTX/DRX. |
| ***cellBarredNTN***Value *barred* means that the cell is barred for connectivity to NTN, as defined in TS 38.304 [20]. Value *notBarred* means that the cell is allowed for connectivity to NTN. If not present, the UE considers the cell is not allowed for connectivity to NTN, as defined in TS 38.304 [20]. This field is only applicable to NTN-capable UEs. |
| ***cellBarredRedCap1Rx***Value *barred* means that the cell is barred for a RedCap UE with 1 Rx branch, as defined in TS 38.304 [20]. This field is ignored by non-RedCap UEs. |
| ***cellBarredRedCap2Rx***Value *barred* means that the cell is barred for a RedCap UE with 2 Rx branches, as defined in TS 38.304 [20]. This field is ignored by non-RedCap UEs. |
| ***cellSelectionInfo***Parameters for cell selection related to the serving cell. |
| ***eCallOverIMS-Support***Indicates whether the cell supports eCall over IMS services as defined in TS 23.501 [32]. If absent, eCall over IMS is not supported by the network in the cell. |
| ***eDRX-AllowedIdle***The presence of this field indicates that extended DRX for CN paging is allowed in the cell for UEs in RRC\_IDLE or RRC\_INACTIVE. The UE shall stop using extended DRX for CN paging in RRC\_IDLE or RRC\_INACTIVE if *eDRX-AllowedIdle* is not present. |
| ***eDRX-AllowedInactive***The presence of *eDRX-AllowedInactive-r17* this field indicates that extended DRX cycle equal to or shorter than 10.24 s for RAN paging is allowed in the cell for UEs in RRC\_INACTIVE. The UE shall stop using extended DRX cycle equal to or shorter than 10.24 s for RAN paging in RRC\_INACTIVE if *eDRX-AllowedInactive-r17* is not present. The presence of *eDRX-AllowedInactive-r18* indicates that extended DRX cycle longer than 10.24 s for RAN paging is allowed in the cell for UEs in RRC\_INACTIVE. The UE shall stop using extended DRX cycle longer than 10.24 s for RAN paging in RRC\_INACTIVE if *eDRX-AllowedInactive-r18* is not present. |
| ***featurePriorities***Indicates priorities for features, such as (e)RedCap, Slicing, SDT, MSG1-Repetitions and MSG3-Repetitions for Coverage Enhancements. These priorities are used to determine which *FeatureCombinationPreambles* the UE shall use when a feature maps to more than one *FeatureCombinationPreambles*, as specified in TS 38.321 [3]. A lower value means a higher priority. The network does not signal the same priority for more than one feature. The network signals a priority for all feature that map to at least one *FeatureCombinationPreambles*. |
| ***halfDuplexRedCap-Allowed***The presence of this field indicates that the cell supports half-duplex FDD (e)RedCap UEs. |
| ***hsdn-Cell***This field indicates this is a HSDN cell as specified in TS 38.304 [20]. |
| ***hyperSFN***Indicates hyper SFN which increments by one when the SFN wraps around. This field is excluded when determining changes in system information, i.e. changes of hyper SFN should not result in system information change notifications. |
| ***idleModeMeasurementsEUTRA***This field indicates that a UE that is configured for EUTRA idle/inactive measurements shall perform the measurements while camping in this cell and report availability of these measurements when establishing or resuming a connection in this cell. If absent, a UE is not required to perform EUTRA idle/inactive measurements. |
| ***idleModeMeasurementsNR***This field indicates that a UE that is configured for NR idle/inactive measurements shall perform the measurements while camping in this cell and report availability of these measurements when establishing or resuming a connection in this cell. If absent, a UE is not required to perform NR idle/inactive measurements. |
| ***ims-EmergencySupport***Indicates whether the cell supports IMS emergency bearer services for UEs in limited service mode. If absent, IMS emergency call is not supported by the network in the cell for UEs in limited service mode. |
| ***intraFreqReselection2RxXR***This field controls cell selection/reselection to intra-frequency cells for 2Rx XR UEs when this cell is barred or treated as barred by the 2Rx XR UE, as specified in TS 38.304 [20]. This field is ignored by all UEs that are not 2Rx XR UEs. This field may be configured only if the cell operates in a frequency band where 4Rx antenna ports are mandated, as specified in TS 38.101-1 [15]. |
| ***intraFreqReselection-eRedCap***Controls cell selection/reselection to intra-frequency cells for eRedCap UEs when this cell is barred, or treated as barred by the eRedCap UE, as specified in TS 38.304 [20]. If not present, an eRedCap UE treats the cell as barred, i.e., the UE considers that the cell does not support eRedCap. |
| ***intraFreqReselectionRedCap***Controls cell selection/reselection to intra-frequency cells for RedCap UEs when this cell is barred, or treated as barred by the RedCap UE, as specified in TS 38.304 [20]. If not present, a RedCap UE treats the cell as barred, i.e.,the UE considers that the cell does not support RedCap. |
| ***mobileIAB-Cell***The presence of this field indicates that this is a mobile IAB cell. |
| ***musim-CapRestrictionAllowed***Indicates the UE is allowed to send the *musim-CapRestrictionInd* in *RRCSetupComplete* and *RRCResumeComplete* messages. |
| ***ncr-Support***This field combines both the support of NCR and the cell status for NCR. If the field is present, the cell supports NCR and the cell is also considered as a candidate for cell (re)selection for NCR-node; if the field is absent, the cell does not support NCR and/or the cell is barred for NCR-node. |
| ***nonServingCellMII***Indicates whether the *MBSInterestIndication* message for MBS broadcast reception on a non-serving cell is allowed to be transmitted to the serving gNB. |
| ***q-QualMin***Parameter "Qqualmin" in TS 38.304 [20], applicable for serving cell. If the field is absent, the UE applies the (default) value of negative infinity for Qqualmin.  |
| ***q-QualMinOffset***Parameter "Qqualminoffset" in TS 38.304 [20]. Actual value Qqualminoffset = field value [dB]. If the field is absent, the UE applies the (default) value of 0 dB for Qqualminoffset.Affects the minimum required quality level in the cell. |
| ***q-RxLevMin***Parameter "Qrxlevmin" in TS 38.304 [20], applicable for serving cell. |
| ***q-RxLevMinOffset***Parameter "Qrxlevminoffset" in TS 38.304 [20]. Actual value Qrxlevminoffset = field value \* 2 [dB]. If absent, the UE applies the (default) value of 0 dB for Qrxlevminoffset*.* Affects the minimum required Rx level in the cell. |
| ***q-RxLevMinSUL***Parameter "Qrxlevmin" in TS 38.304 [20], applicable for serving cell. |
| ***sdt-DataVolumeThreshold***Data volume threshold used to determine whether SDT can be initiated, as specified in TS 38.321 [3]. Value *byte32* corresponds to 32 bytes, value *byte100* corresponds to 100 bytes, and so on. |
| ***sdt-LogicalChannelSR-DelayTimer***The value of *logicalChannelSR-DelayTimer* applied during SDT for logical channels configured with SDT, as specified in TS 38.321 [3]. Value in number of subframes. Value *sf20* corresponds to 20 subframes, *sf40* corresponds to 40 subframes, and so on. If *sdt-LogicalChannelSR-DelayTimer-r18* is absent and *sdt-LogicalChannelSR-DelayTimer-r17* is present then, the UE applies the value configured in *sdt-LogicalChannelSR-DelayTimer-r17* for this field. If this field is not configured, then logicalChannelSR-DelayTimer is not applied for SDT logical channels. |
| ***sdt-RSRP-Threshold***RSRP threshold used to determine whether SDT procedure can be initiated, as specified in TS 38.321 [3]. |
| ***sdt-RSRP-ThresholdMT***RSRP threshold used to determine whether MT-SDT procedure can be initiated, as specified in TS 38.321 [3]. If the field is absent, and the field *sdt-RSRP-Threshold* is present, the UE applies the value in the field *sdt-RSRP-Threshold*. |
| ***servingCellConfigCommon***Configuration of the serving cell. |
| ***t319a***Initial value of the timer T319a used for detection of SDT failure. Value *ms100* corresponds to 100 milliseconds, value *ms200* corresponds to 200 milliseconds and so on. If *t319a-r18* is absent, the UE applies the value configured in *t319a-r17.* |
| ***uac-AccessCategory1-SelectionAssistanceInfo***Information used to determine whether Access Category 1 applies to the UE, as defined in TS 22.261 [25]. If *plmnCommon* is chosen, the *UAC-AccessCategory1-SelectionAssistanceInfo* is applicable to all the PLMNs and SNPNs in *plmn-IdentityInfoList* and *npn-IdentityInfoList*. If *individualPLMNList* is chosen, the 1st entry in the list corresponds to the first network within all of the PLMNs and SNPNs across the *plmn-IdentityList* and the *npn-IdentityInfoList*, the 2nd entry in the list corresponds to the second network within all of the PLMNs and SNPNs across the *plmn-IdentityList* and the *npn-IdentityInfoList* and so on. If *uac-AC1-SelectAssistInfo-r16* is present, the UE shall ignore the *uac-AccessCategory1-SelectionAssistanceInfo*. |
| ***uac-AC1-SelectAssistInfo***Information used to determine whether Access Category 1 applies to the UE, as defined in TS 22.261 [25]. The 1st entry in the list corresponds to the first network within all of the PLMNs and SNPNs across the *plmn-IdentityList* and *npn-IdentityInfoList*, the 2nd entry in the list corresponds to the second network within all of the PLMNs and SNPNs across the *plmn-IdentityList* and the *npn-IdentityInfoList* and so on. Value *notConfigured* indicates that Access Category1 is not configured for the corresponding PLMN/SNPN. |
| ***uac-BarringForCommon***Common access control parameters for each access category. Common values are used for all PLMNs/SNPNs, unless overwritten by the PLMN/SNPN specific configuration provided in *uac-BarringPerPLMN-List*. The parameters are specified by providing an index to the set of configurations (*uac-BarringInfoSetList*). UE behaviour upon absence of this field is specified in clause 5.3.14.2. |
| ***ue-TimersAndConstants***Timer and constant values to be used by the UE. The cell operating as PCell always provides this field. |
| ***useFullResumeID***Indicates which resume identifier and Resume request message should be used. UE uses *fullI-RNTI* and *RRCResumeRequest1* if the field is present, or *shortI-RNTI* and *RRCResumeRequest* if the field is absent. |

|  |  |
| --- | --- |
| Conditional Presence | Explanation |
| *EDRX-RC* | The field is optionally present, Need R, in a cell that enables *eDRX-AllowedIdle*, otherwise it is absent. |
| *MINT* | The field is optionally present, Need R, in a cell that provides a configuration for disaster roaming, otherwise it is absent, Need R. |
| *MT-SDT1* | This field is optionally present, Need S, in a cell that supports MT-SDT if *sdt-ConfigCommon-r17* is not present, otherwise it is absent. |
| *MT-SDT2* | This field is mandatory present in a cell that supports MT-SDT if *sdt-ConfigCommon-r17* is not present, otherwise it is absent. |
| *Standalone* | The field is mandatory present in a cell that supports standalone operation, otherwise it is absent. |

### 6.3.1 System information blocks

#### – *SIB4*

*SIB4* contains information relevant for inter-frequency cell re-selection (i.e. information about other NR frequencies and inter-frequency neighbouring cells relevant for cell re-selection), which can also be used for NR idle/inactive measurements. The IE includes cell re-selection parameters common for a frequency as well as cell specific re-selection parameters.

*SIB4* information element

-- ASN1START

-- TAG-SIB4-START

SIB4 ::= SEQUENCE {

 interFreqCarrierFreqList InterFreqCarrierFreqList,

 lateNonCriticalExtension OCTET STRING OPTIONAL,

 ...,

 [[

 interFreqCarrierFreqList-v1610 InterFreqCarrierFreqList-v1610 OPTIONAL -- Need R

 ]],

 [[

 interFreqCarrierFreqList-v1700 InterFreqCarrierFreqList-v1700 OPTIONAL -- Need R

 ]],

 [[

 interFreqCarrierFreqList-v1720 InterFreqCarrierFreqList-v1720 OPTIONAL -- Need R

 ]],

 [[

 interFreqCarrierFreqList-v1730 InterFreqCarrierFreqList-v1730 OPTIONAL -- Need R

 ]],

 [[

 interFreqCarrierFreqList-v1760 InterFreqCarrierFreqList-v1760 OPTIONAL -- Need R

 ]],

 [[

 interFreqCarrierFreqList-v1800 InterFreqCarrierFreqList-v1800 OPTIONAL -- Need R

 ]]

}

InterFreqCarrierFreqList ::= SEQUENCE (SIZE (1..maxFreq)) OF InterFreqCarrierFreqInfo

InterFreqCarrierFreqList-v1610 ::= SEQUENCE (SIZE (1..maxFreq)) OF InterFreqCarrierFreqInfo-v1610

InterFreqCarrierFreqList-v1700 ::= SEQUENCE (SIZE (1..maxFreq)) OF InterFreqCarrierFreqInfo-v1700

InterFreqCarrierFreqList-v1720 ::= SEQUENCE (SIZE (1..maxFreq)) OF InterFreqCarrierFreqInfo-v1720

InterFreqCarrierFreqList-v1730 ::= SEQUENCE (SIZE (1..maxFreq)) OF InterFreqCarrierFreqInfo-v1730

InterFreqCarrierFreqList-v1760 ::= SEQUENCE (SIZE (1..maxFreq)) OF InterFreqCarrierFreqInfo-v1760

InterFreqCarrierFreqList-v1800 ::= SEQUENCE (SIZE (1..maxFreq)) OF InterFreqCarrierFreqInfo-v1800

InterFreqCarrierFreqInfo ::= SEQUENCE {

 dl-CarrierFreq ARFCN-ValueNR,

 frequencyBandList MultiFrequencyBandListNR-SIB OPTIONAL, -- Cond Mandatory

 frequencyBandListSUL MultiFrequencyBandListNR-SIB OPTIONAL, -- Need R

 nrofSS-BlocksToAverage INTEGER (2..maxNrofSS-BlocksToAverage) OPTIONAL, -- Need S

 absThreshSS-BlocksConsolidation ThresholdNR OPTIONAL, -- Need S

 smtc SSB-MTC OPTIONAL, -- Need S

 ssbSubcarrierSpacing SubcarrierSpacing,

 ssb-ToMeasure SSB-ToMeasure OPTIONAL, -- Need S

 deriveSSB-IndexFromCell BOOLEAN,

 ss-RSSI-Measurement SS-RSSI-Measurement OPTIONAL, -- Need R

 q-RxLevMin Q-RxLevMin,

 q-RxLevMinSUL Q-RxLevMin OPTIONAL, -- Need R

 q-QualMin Q-QualMin OPTIONAL, -- Need S

 p-Max P-Max OPTIONAL, -- Need S

 t-ReselectionNR T-Reselection,

 t-ReselectionNR-SF SpeedStateScaleFactors OPTIONAL, -- Need S

 threshX-HighP ReselectionThreshold,

 threshX-LowP ReselectionThreshold,

 threshX-Q SEQUENCE {

 threshX-HighQ ReselectionThresholdQ,

 threshX-LowQ ReselectionThresholdQ

 } OPTIONAL, -- Cond RSRQ

 cellReselectionPriority CellReselectionPriority OPTIONAL, -- Need R

 cellReselectionSubPriority CellReselectionSubPriority OPTIONAL, -- Need R

 q-OffsetFreq Q-OffsetRange DEFAULT dB0,

 interFreqNeighCellList InterFreqNeighCellList OPTIONAL, -- Need R

 interFreqExcludedCellList InterFreqExcludedCellList OPTIONAL, -- Need R

 ...,

 [[

 mobileIAB-Freq ENUMERATED {true} OPTIONAL -- Need R

 ]]

}

InterFreqCarrierFreqInfo-v1610 ::= SEQUENCE {

 interFreqNeighCellList-v1610 InterFreqNeighCellList-v1610 OPTIONAL, -- Need R

 smtc2-LP-r16 SSB-MTC2-LP-r16 OPTIONAL, -- Need R

 interFreqAllowedCellList-r16 InterFreqAllowedCellList-r16 OPTIONAL, -- Cond SharedSpectrum2

 ssb-PositionQCL-Common-r16 SSB-PositionQCL-Relation-r16 OPTIONAL, -- Cond SharedSpectrum

 interFreqCAG-CellList-r16 SEQUENCE (SIZE (1..maxPLMN)) OF InterFreqCAG-CellListPerPLMN-r16 OPTIONAL -- Need R

}

InterFreqCarrierFreqInfo-v1700 ::= SEQUENCE {

 interFreqNeighHSDN-CellList-r17 InterFreqNeighHSDN-CellList-r17 OPTIONAL, -- Need R

 highSpeedMeasInterFreq-r17 ENUMERATED {true} OPTIONAL, -- Need R

 redCapAccessAllowed-r17 ENUMERATED {true} OPTIONAL, -- Need R

 ssb-PositionQCL-Common-r17 SSB-PositionQCL-Relation-r17 OPTIONAL, -- Cond SharedSpectrum

 interFreqNeighCellList-v1710 InterFreqNeighCellList-v1710 OPTIONAL -- Cond SharedSpectrum2

}

InterFreqCarrierFreqInfo-v1720 ::= SEQUENCE {

 smtc4list-r17 SSB-MTC4List-r17 OPTIONAL -- Need R

}

InterFreqCarrierFreqInfo-v1730 ::= SEQUENCE {

 channelAccessMode2-r17 ENUMERATED {enabled} OPTIONAL -- Need R

}

InterFreqCarrierFreqInfo-v1760 ::= SEQUENCE {

 frequencyBandList-v1760 MultiFrequencyBandListNR-SIB-v1760 OPTIONAL, -- Need R

 frequencyBandListSUL-v1760 MultiFrequencyBandListNR-SIB-v1760 OPTIONAL -- Need R

}

InterFreqCarrierFreqInfo-v1800 ::= SEQUENCE {

 frequencyBandListAerial-r18 MultiFrequencyBandListNR-Aerial-SIB-r18 OPTIONAL, -- Need S

 mobileIAB-CellList-r18 PCI-Range OPTIONAL, -- Need R

 eRedCapAccessAllowed-r18 ENUMERATED {true} OPTIONAL, -- Need R

 tn-AreaIdList-r18 SEQUENCE (SIZE (1..maxTN-AreaInfo-r18)) OF TN-AreaId-r18 OPTIONAL, -- Need R

 accessAllowed2RxXR-r18 ENUMERATED {true} OPTIONAL -- Need R

}

InterFreqNeighHSDN-CellList-r17 ::= SEQUENCE (SIZE (1..maxCellInter)) OF PCI-Range

InterFreqNeighCellList ::= SEQUENCE (SIZE (1..maxCellInter)) OF InterFreqNeighCellInfo

InterFreqNeighCellList-v1610 ::= SEQUENCE (SIZE (1..maxCellInter)) OF InterFreqNeighCellInfo-v1610

InterFreqNeighCellList-v1710 ::= SEQUENCE (SIZE (1..maxCellInter)) OF InterFreqNeighCellInfo-v1710

InterFreqNeighCellInfo ::= SEQUENCE {

 physCellId PhysCellId,

 q-OffsetCell Q-OffsetRange,

 q-RxLevMinOffsetCell INTEGER (1..8) OPTIONAL, -- Need R

 q-RxLevMinOffsetCellSUL INTEGER (1..8) OPTIONAL, -- Need R

 q-QualMinOffsetCell INTEGER (1..8) OPTIONAL, -- Need R

 ...

}

InterFreqNeighCellInfo-v1610 ::= SEQUENCE {

 ssb-PositionQCL-r16 SSB-PositionQCL-Relation-r16 OPTIONAL -- Cond SharedSpectrum2

}

InterFreqNeighCellInfo-v1710 ::= SEQUENCE {

 ssb-PositionQCL-r17 SSB-PositionQCL-Relation-r17 OPTIONAL -- Cond SharedSpectrum2

}

InterFreqExcludedCellList ::= SEQUENCE (SIZE (1..maxCellExcluded)) OF PCI-Range

InterFreqAllowedCellList-r16 ::= SEQUENCE (SIZE (1..maxCellAllowed)) OF PCI-Range

InterFreqCAG-CellListPerPLMN-r16 ::= SEQUENCE {

 plmn-IdentityIndex-r16 INTEGER (1..maxPLMN),

 cag-CellList-r16 SEQUENCE (SIZE (1..maxCAG-Cell-r16)) OF PCI-Range

}

-- TAG-SIB4-STOP

-- ASN1STOP

| *SIB4* field descriptions |
| --- |
| ***absThreshSS-BlocksConsolidation***Threshold for consolidation of L1 measurements per RS index. If the field is absent, the UE uses the measurement quantity as specified in TS 38.304 [20]. |
| ***accessAllowed2RxXR***Indicates if the cells on the frequency support 2Rx XR UEs. If present, 2Rx XR UEs shall consider only these NR frequencies in cell reselection evaluation. |
| ***channelAccessMode2***If present, this field indicates that the neighbor cells on the inter-frequency apply channel access mode procedures for operation with shared spectrum channel access in accordance with TS 37.213 [48], clause 4.4 for FR2-2. If absent, the neighbor cells on the inter-frequency do not apply any channel access procedure. |
| ***deriveSSB-IndexFromCell***This field indicates whether the UE may use the timing of any detected cell on that frequency to derive the SSB index of all neighbour cells on that frequency. If this field is set to *true*, the UE assumes SFN and frame boundary alignment across cells on the neighbor frequency as specified in TS 38.133 [14]. |
| ***dl-CarrierFreq***This field indicates center frequency of the SS block of the neighbour cells, where the frequency corresponds to a GSCN value as specified in TS 38.101-1 [15] or TS 38.101-5 [75]. |
| ***eRedCapAccessAllowed***Indicates whether eRedCap UEs are allowed to access cells on the frequency. |
| ***frequencyBandList***Indicates the list of frequency bands for which the NR cell reselection parameters apply. |
| ***frequencyBandListAerial***Indicates the list of frequency bands for aerial operation for which the NR cell reselection parameters apply. The UE behaviour in case the field is absent is described in clause 5.2.2.4.5. |
| ***highSpeedMeasInterFreq***If the field is set to *true* and UE supports high speed inter-frequency IDLE/INACTIVE measurements, the UE shall apply the enhanced inter-frequency RRM requirements on the inter-frequency carrier to support high speed up to 500 km/h in RRC\_IDLE/RRC\_INACTIVE as specified in TS 38.133 [14]. |
| ***interFreqAllowedCellList***List of allow-listed inter-frequency neighbouring cells, see TS 38.304 [20], clause 5.2.4. |
| ***interFreqCAG-CellList***List of inter-frequency neighbouring CAG cells (as defined in TS 38.304 [20] per PLMN. |
| ***interFreqCarrierFreqList***List of neighbouring carrier frequencies and frequency specific cell re-selection information. If *interFreqCarrierFreqList-v1610, interFreqCarrierFreqList-v1700, interFreqCarrierFreqList-v1720*, *interFreqCarrierFreqList-v1730,* *interFreqCarrierFreqList-v1760* or *InterFreqCarrierFreqInfo-v1800* are present, they shall contain the same number of entries, listed in the same order as in *interFreqCarrierFreqList* (without suffix). |
| ***interFreqExcludedCellList***List of exclude-listed inter-frequency neighbouring cells. |
| ***interFreqNeighCellList***List of inter-frequency neighbouring cells with specific cell re-selection parameters. If *interFreqNeighCellList-v1610* is present, it shall contain the same number of entries, listed in the same order as in *interFreqNeighCellList* (without suffix). |
| ***interFreqNeighHSDN-CellList***List of inter-frequency neighbouring HSDN cells as specified in TS 38.304 [20]. |
| ***mobileIAB-CellList***Contains a PCI range on which mobile IAB cells may be deployed. |
| ***mobileIAB-Freq***If present, it indicates that a mobile IAB node may deployed on the inter-frequency carrier. |
| ***nrofSS-BlocksToAverage***Number of SS blocks to average for cell measurement derivation. If the field is absent, the UE uses the measurement quantity as specified in TS 38.304 [20]. |
| ***p-Max***Value in dBm applicable for the neighbouring NR cells on this carrier frequency. If absent the UE applies the maximum power according to TS 38.101-1 [15] in case of an FR1 cell, TS 38.101-2 [39] in case of an FR2 cell or TS 38.101-5 [75] in case of an NTN cell. In this release of the specification, if *p-Max* is present on a carrier frequency in FR2, the UE shall ignore the field and applies the maximum power according to TS 38.101-2 [39]. This field is ignored by IAB-MT. The IAB-MT applies output power and emissions requirements, as specified in TS 38.174 [63]. |
| ***q-OffsetCell***Parameter "Qoffsets,n" in TS 38.304 [20]. |
| ***q-OffsetFreq***Parameter "Qoffsetfrequency" in TS 38.304 [20]. |
| ***q-QualMin***Parameter "Qqualmin" in TS 38.304 [20]. If the field is absent, the UE applies the (default) value of negative infinity for Qqualmin. |
| ***q-QualMinOffsetCell***Parameter "Qqualminoffsetcell" in TS 38.304 [20]. Actual value Qqualminoffsetcell = field value [dB]. |
| ***q-RxLevMin***Parameter "Qrxlevmin" in TS 38.304 [20]. |
| ***q-RxLevMinOffsetCell***Parameter "Qrxlevminoffsetcell" in TS 38.304 [20]. Actual value Qrxlevminoffsetcell = field value \* 2 [dB]. |
| ***q-RxLevMinOffsetCellSUL***Parameter "QrxlevminoffsetcellSUL" in TS 38.304 [20]. Actual value QrxlevminoffsetcellSUL = field value \* 2 [dB]. |
| ***q-RxLevMinSUL***Parameter "Qrxlevmin" in TS 38.304 [20]. |
| ***redCapAccessAllowed***Indicates whether RedCap UEs are allowed to access cells on the frequency. |
| ***smtc***Measurement timing configuration for inter-frequency measurement. If this field is absent, the UE assumes that SSB periodicity is 5 ms in this frequency. If the field is broadcast by an NTN cell, the o*ffset* (derived from parameter *periodicityAndOffset*) is based on the assumption that the gNB-UE propagation delay difference between the serving cell and neighbour cells equals to 0 ms, and UE can adjust the actual o*ffset* based on the actual propagation delay difference. |
| ***smtc2-LP***Measurement timing configuration for inter-frequency neighbour cells with a Long Periodicity (LP) indicated by periodicity in *smtc2-LP*. The timing offset and duration are equal to the offset and duration indicated in *smtc* in *InterFreqCarrierFreqInfo*. The periodicity in *smtc2-LP* can only be set to a value strictly larger than the periodicity in *smtc* in *InterFreqCarrierFreqInfo* (e.g. if *smtc* indicates sf20 the Long Periodicity can only be set to sf40, sf80 or sf160, if *smtc* indicates sf160, *smtc2-LP* cannot be configured). The *pci-List*, if present, includes the physical cell identities of the inter-frequency neighbour cells with Long Periodicity. If *smtc2-LP* is absent, the UE assumes that there are no inter-frequency neighbour cells with a Long Periodicity. |
| ***smtc4list***Measurement timing configuration list for NTN deployments, see clause 5.5.2.10. The offset of each SSB-MTC4 in *smtc4list* is based on the assumption that the gNB-UE propagation delay difference between the serving cell and neighbour cells equals to 0 ms, and UE can adjust the actual *offset* based on the actual propagation delay difference. For a UE that supports less SMTCs than what is included in this list, it is up to the UE to select which SMTCs to consider. |
| ***ssb-PositionQCL***Indicates the QCL relation between SS/PBCH blocks for a specific neighbor cell as specified in TS 38.213 [13], clause 4.1. If provided, the cell specific value overwrites the common value signalled by *ssb-PositionQCL-Common* in *SIB4* for the indicated cell. |
| ***ssb-PositionQCL-Common***Indicates the QCL relation between SS/PBCH blocks for inter-frequency neighbor cells as specified in TS 38.213 [13], clause 4.1. |
| ***ssb-ToMeasure***The set of SS blocks to be measured within the SMTC measurement duration (see TS 38.215 [9]). When the field is absent the UE measures on all SS-blocks. |
| ***ssbSubcarrierSpacing***Subcarrier spacing of SSB.Only the following values are applicable depending on the used frequency:FR1: 15 or 30 kHzFR2-1: 120 or 240 kHzFR2-2: 120, 480, or 960 kHz |
| ***threshX-HighP***Parameter "ThreshX, HighP" in TS 38.304 [20]. |
| ***threshX-HighQ***Parameter "ThreshX, HighQ" in TS 38.304 [20]. |
| ***threshX-LowP***Parameter "ThreshX, LowP" in TS 38.304 [20]. |
| ***threshX-LowQ***Parameter "ThreshX, LowQ" in TS 38.304 [20]. |
| ***t-ReselectionNR***Parameter "TreselectionNR" in TS 38.304 [20]. |
| ***t-ReselectionNR-SF***Parameter "Speed dependent ScalingFactor for TreselectionNR" in TS 38.304 [20]. If the field is absent, the UE behaviour is specified in TS 38.304 [20]. |

|  |  |
| --- | --- |
| Conditional Presence | Explanation |
| *Mandatory* | The field is mandatory present in SIB4. |
| *RSRQ* | The field is mandatory present if *threshServingLowQ* is present in *SIB2*; otherwise it is absent. |
| *SharedSpectrum* | This field is mandatory present if this inter-frequency operates with shared spectrum channel access. Otherwise, it is absent, Need R. |
| *SharedSpectrum2* | The field is optional present, Need R, if this inter-frequency or neighbor cell operates with shared spectrum channel access. Otherwise, it is absent, Need R. |

### 6.3.3 UE capability information elements

#### – *RF-Parameters*

The IE *RF-Parameters* is used to convey RF-related capabilities for NR operation.

*RF-Parameters* information element

-- ASN1START

-- TAG-RF-PARAMETERS-START

RF-Parameters ::= SEQUENCE {

 supportedBandListNR SEQUENCE (SIZE (1..maxBands)) OF BandNR,

 supportedBandCombinationList BandCombinationList OPTIONAL,

 appliedFreqBandListFilter FreqBandList OPTIONAL,

 ...,

 [[

 supportedBandCombinationList-v1540 BandCombinationList-v1540 OPTIONAL,

 srs-SwitchingTimeRequested ENUMERATED {true} OPTIONAL

 ]],

 [[

 supportedBandCombinationList-v1550 BandCombinationList-v1550 OPTIONAL

 ]],

 [[

 supportedBandCombinationList-v1560 BandCombinationList-v1560 OPTIONAL

 ]],

 [[

 supportedBandCombinationList-v1610 BandCombinationList-v1610 OPTIONAL,

 supportedBandCombinationListSidelinkEUTRA-NR-r16 BandCombinationListSidelinkEUTRA-NR-r16 OPTIONAL,

 supportedBandCombinationList-UplinkTxSwitch-r16 BandCombinationList-UplinkTxSwitch-r16 OPTIONAL

 ]],

 [[

 supportedBandCombinationList-v1630 BandCombinationList-v1630 OPTIONAL,

 supportedBandCombinationListSidelinkEUTRA-NR-v1630 BandCombinationListSidelinkEUTRA-NR-v1630 OPTIONAL,

 supportedBandCombinationList-UplinkTxSwitch-v1630 BandCombinationList-UplinkTxSwitch-v1630 OPTIONAL

 ]],

 [[

 supportedBandCombinationList-v1640 BandCombinationList-v1640 OPTIONAL,

 supportedBandCombinationList-UplinkTxSwitch-v1640 BandCombinationList-UplinkTxSwitch-v1640 OPTIONAL

 ]],

 [[

 supportedBandCombinationList-v1650 BandCombinationList-v1650 OPTIONAL,

 supportedBandCombinationList-UplinkTxSwitch-v1650 BandCombinationList-UplinkTxSwitch-v1650 OPTIONAL

 ]],

 [[

 extendedBand-n77-r16 ENUMERATED {supported} OPTIONAL

 ]],

 [[

 supportedBandCombinationList-UplinkTxSwitch-v1670 BandCombinationList-UplinkTxSwitch-v1670 OPTIONAL

 ]],

 [[

 supportedBandCombinationList-v1680 BandCombinationList-v1680 OPTIONAL

 ]],

 [[

 supportedBandCombinationList-v1690 BandCombinationList-v1690 OPTIONAL,

 supportedBandCombinationList-UplinkTxSwitch-v1690 BandCombinationList-UplinkTxSwitch-v1690 OPTIONAL

 ]],

 [[

 supportedBandCombinationList-v1700 BandCombinationList-v1700 OPTIONAL,

 supportedBandCombinationList-UplinkTxSwitch-v1700 BandCombinationList-UplinkTxSwitch-v1700 OPTIONAL,

 supportedBandCombinationListSL-RelayDiscovery-r17 OCTET STRING OPTIONAL, -- Contains PC5 BandCombinationListSidelinkNR-r16

 supportedBandCombinationListSL-NonRelayDiscovery-r17 OCTET STRING OPTIONAL, -- Contains PC5 BandCombinationListSidelinkNR-r16

 supportedBandCombinationListSidelinkEUTRA-NR-v1710 BandCombinationListSidelinkEUTRA-NR-v1710 OPTIONAL,

 sidelinkRequested-r17 ENUMERATED {true} OPTIONAL,

 extendedBand-n77-2-r17 ENUMERATED {supported} OPTIONAL

 ]],

 [[

 supportedBandCombinationList-v1720 BandCombinationList-v1720 OPTIONAL,

 supportedBandCombinationList-UplinkTxSwitch-v1720 BandCombinationList-UplinkTxSwitch-v1720 OPTIONAL

 ]],

 [[

 supportedBandCombinationList-v1730 BandCombinationList-v1730 OPTIONAL,

 supportedBandCombinationList-UplinkTxSwitch-v1730 BandCombinationList-UplinkTxSwitch-v1730 OPTIONAL,

 supportedBandCombinationListSL-RelayDiscovery-v1730 BandCombinationListSL-Discovery-r17 OPTIONAL,

 supportedBandCombinationListSL-NonRelayDiscovery-v1730 BandCombinationListSL-Discovery-r17 OPTIONAL

 ]],

 [[

 supportedBandCombinationList-v1740 BandCombinationList-v1740 OPTIONAL,

 supportedBandCombinationList-UplinkTxSwitch-v1740 BandCombinationList-UplinkTxSwitch-v1740 OPTIONAL

 ]],

 [[

 supportedBandCombinationList-v1760 BandCombinationList-v1760 OPTIONAL,

 supportedBandCombinationList-UplinkTxSwitch-v1760 BandCombinationList-UplinkTxSwitch-v1760 OPTIONAL

 ]],

 [[

 supportedBandCombinationList-v1770 BandCombinationList-v1770 OPTIONAL,

 supportedBandCombinationList-UplinkTxSwitch-v1770 BandCombinationList-UplinkTxSwitch-v1770 OPTIONAL

 ]],

 [[

 supportedBandCombinationList-v1800 BandCombinationList-v1800 OPTIONAL,

 supportedBandCombinationList-UplinkTxSwitch-v1800 BandCombinationList-UplinkTxSwitch-v1800 OPTIONAL,

 supportedBandCombinationListSL-U2U-Relay-r18 SEQUENCE {

 supportedBandCombinationListSL-U2U-RelayDiscovery-r18 OCTET STRING OPTIONAL, -- Contains PC5

 -- BandCombinationListSidelinkNR-r16

 supportedBandCombinationListSL-U2U-DiscoveryExt BandCombinationListSL-Discovery-r17 OPTIONAL

 } OPTIONAL

 ]]

}

RF-Parameters-v15g0 ::= SEQUENCE {

 supportedBandCombinationList-v15g0 BandCombinationList-v15g0 OPTIONAL

}

RF-Parameters-v16a0 ::= SEQUENCE {

 supportedBandCombinationList-v16a0 BandCombinationList-v16a0 OPTIONAL,

 supportedBandCombinationList-UplinkTxSwitch-v16a0 BandCombinationList-UplinkTxSwitch-v16a0 OPTIONAL

}

RF-Parameters-v16c0 ::= SEQUENCE {

 supportedBandListNR-v16c0 SEQUENCE (SIZE (1..maxBands)) OF BandNR-v16c0

}

BandNR ::= SEQUENCE {

 bandNR FreqBandIndicatorNR,

 modifiedMPR-Behaviour BIT STRING (SIZE (8)) OPTIONAL,

 mimo-ParametersPerBand MIMO-ParametersPerBand OPTIONAL,

 extendedCP ENUMERATED {supported} OPTIONAL,

 multipleTCI ENUMERATED {supported} OPTIONAL,

 bwp-WithoutRestriction ENUMERATED {supported} OPTIONAL,

 bwp-SameNumerology ENUMERATED {upto2, upto4} OPTIONAL,

 bwp-DiffNumerology ENUMERATED {upto4} OPTIONAL,

 crossCarrierScheduling-SameSCS ENUMERATED {supported} OPTIONAL,

 pdsch-256QAM-FR2 ENUMERATED {supported} OPTIONAL,

 pusch-256QAM ENUMERATED {supported} OPTIONAL,

 ue-PowerClass ENUMERATED {pc1, pc2, pc3, pc4} OPTIONAL,

 rateMatchingLTE-CRS ENUMERATED {supported} OPTIONAL,

 channelBWs-DL CHOICE {

 fr1 SEQUENCE {

 scs-15kHz BIT STRING (SIZE (10)) OPTIONAL,

 scs-30kHz BIT STRING (SIZE (10)) OPTIONAL,

 scs-60kHz BIT STRING (SIZE (10)) OPTIONAL

 },

 fr2 SEQUENCE {

 scs-60kHz BIT STRING (SIZE (3)) OPTIONAL,

 scs-120kHz BIT STRING (SIZE (3)) OPTIONAL

 }

 } OPTIONAL,

 channelBWs-UL CHOICE {

 fr1 SEQUENCE {

 scs-15kHz BIT STRING (SIZE (10)) OPTIONAL,

 scs-30kHz BIT STRING (SIZE (10)) OPTIONAL,

 scs-60kHz BIT STRING (SIZE (10)) OPTIONAL

 },

 fr2 SEQUENCE {

 scs-60kHz BIT STRING (SIZE (3)) OPTIONAL,

 scs-120kHz BIT STRING (SIZE (3)) OPTIONAL

 }

 } OPTIONAL,

 ...,

 [[

 maxUplinkDutyCycle-PC2-FR1 ENUMERATED {n60, n70, n80, n90, n100} OPTIONAL

 ]],

 [[

 pucch-SpatialRelInfoMAC-CE ENUMERATED {supported} OPTIONAL,

 powerBoosting-pi2BPSK ENUMERATED {supported} OPTIONAL

 ]],

 [[

 maxUplinkDutyCycle-FR2 ENUMERATED {n15, n20, n25, n30, n40, n50, n60, n70, n80, n90, n100} OPTIONAL

 ]],

 [[

 channelBWs-DL-v1590 CHOICE {

 fr1 SEQUENCE {

 scs-15kHz BIT STRING (SIZE (16)) OPTIONAL,

 scs-30kHz BIT STRING (SIZE (16)) OPTIONAL,

 scs-60kHz BIT STRING (SIZE (16)) OPTIONAL

 },

 fr2 SEQUENCE {

 scs-60kHz BIT STRING (SIZE (8)) OPTIONAL,

 scs-120kHz BIT STRING (SIZE (8)) OPTIONAL

 }

 } OPTIONAL,

 channelBWs-UL-v1590 CHOICE {

 fr1 SEQUENCE {

 scs-15kHz BIT STRING (SIZE (16)) OPTIONAL,

 scs-30kHz BIT STRING (SIZE (16)) OPTIONAL,

 scs-60kHz BIT STRING (SIZE (16)) OPTIONAL

 },

 fr2 SEQUENCE {

 scs-60kHz BIT STRING (SIZE (8)) OPTIONAL,

 scs-120kHz BIT STRING (SIZE (8)) OPTIONAL

 }

 } OPTIONAL

 ]],

 [[

 asymmetricBandwidthCombinationSet BIT STRING (SIZE (1..32)) OPTIONAL

 ]],

 [[

 -- R1 10: NR-unlicensed

 sharedSpectrumChAccessParamsPerBand-r16 SharedSpectrumChAccessParamsPerBand-r16 OPTIONAL,

 -- R1 11-7b: Independent cancellation of the overlapping PUSCHs in an intra-band UL CA

 cancelOverlappingPUSCH-r16 ENUMERATED {supported} OPTIONAL,

 -- R1 14-1: Multiple LTE-CRS rate matching patterns

 multipleRateMatchingEUTRA-CRS-r16 SEQUENCE {

 maxNumberPatterns-r16 INTEGER (2..6),

 maxNumberNon-OverlapPatterns-r16 INTEGER (1..3)

 } OPTIONAL,

 -- R1 14-1a: Two LTE-CRS overlapping rate matching patterns within a part of NR carrier using 15 kHz overlapping with a LTE carrier

 overlapRateMatchingEUTRA-CRS-r16 ENUMERATED {supported} OPTIONAL,

 -- R1 14-2: PDSCH Type B mapping of length 9 and 10 OFDM symbols

 pdsch-MappingTypeB-Alt-r16 ENUMERATED {supported} OPTIONAL,

 -- R1 14-3: One slot periodic TRS configuration for FR1

 oneSlotPeriodicTRS-r16 ENUMERATED {supported} OPTIONAL,

 olpc-SRS-Pos-r16 OLPC-SRS-Pos-r16 OPTIONAL,

 spatialRelationsSRS-Pos-r16 SpatialRelationsSRS-Pos-r16 OPTIONAL,

 simulSRS-MIMO-TransWithinBand-r16 ENUMERATED {n2} OPTIONAL,

 channelBW-DL-IAB-r16 CHOICE {

 fr1-100mhz SEQUENCE {

 scs-15kHz ENUMERATED {supported} OPTIONAL,

 scs-30kHz ENUMERATED {supported} OPTIONAL,

 scs-60kHz ENUMERATED {supported} OPTIONAL

 },

 fr2-200mhz SEQUENCE {

 scs-60kHz ENUMERATED {supported} OPTIONAL,

 scs-120kHz ENUMERATED {supported} OPTIONAL

 }

 } OPTIONAL,

 channelBW-UL-IAB-r16 CHOICE {

 fr1-100mhz SEQUENCE {

 scs-15kHz ENUMERATED {supported} OPTIONAL,

 scs-30kHz ENUMERATED {supported} OPTIONAL,

 scs-60kHz ENUMERATED {supported} OPTIONAL

 },

 fr2-200mhz SEQUENCE {

 scs-60kHz ENUMERATED {supported} OPTIONAL,

 scs-120kHz ENUMERATED {supported} OPTIONAL

 }

 } OPTIONAL,

 rasterShift7dot5-IAB-r16 ENUMERATED {supported} OPTIONAL,

 ue-PowerClass-v1610 ENUMERATED {pc1dot5} OPTIONAL,

 condHandover-r16 ENUMERATED {supported} OPTIONAL,

 condHandoverFailure-r16 ENUMERATED {supported} OPTIONAL,

 condHandoverTwoTriggerEvents-r16 ENUMERATED {supported} OPTIONAL,

 condPSCellChange-r16 ENUMERATED {supported} OPTIONAL,

 condPSCellChangeTwoTriggerEvents-r16 ENUMERATED {supported} OPTIONAL,

 mpr-PowerBoost-FR2-r16 ENUMERATED {supported} OPTIONAL,

 -- R1 11-9: Multiple active configured grant configurations for a BWP of a serving cell

 activeConfiguredGrant-r16 SEQUENCE {

 maxNumberConfigsPerBWP-r16 ENUMERATED {n1, n2, n4, n8, n12},

 maxNumberConfigsAllCC-r16 INTEGER (2..32)

 } OPTIONAL,

 -- R1 11-9a: Joint release in a DCI for two or more configured grant Type 2 configurations for a given BWP of a serving cell

 jointReleaseConfiguredGrantType2-r16 ENUMERATED {supported} OPTIONAL,

 -- R1 12-2: Multiple SPS configurations

 sps-r16 SEQUENCE {

 maxNumberConfigsPerBWP-r16 INTEGER (1..8),

 maxNumberConfigsAllCC-r16 INTEGER (2..32)

 } OPTIONAL,

 -- R1 12-2a: Joint release in a DCI for two or more SPS configurations for a given BWP of a serving cell

 jointReleaseSPS-r16 ENUMERATED {supported} OPTIONAL,

 -- R1 13-19: Simultaneous positioning SRS and MIMO SRS transmission within a band across multiple CCs

 simulSRS-TransWithinBand-r16 ENUMERATED {n2} OPTIONAL,

 trs-AdditionalBandwidth-r16 ENUMERATED {trs-AddBW-Set1, trs-AddBW-Set2} OPTIONAL,

 handoverIntraF-IAB-r16 ENUMERATED {supported} OPTIONAL

 ]],

 [[

 -- R1 22-5a: Simultaneous transmission of SRS for antenna switching and SRS for CB/NCB /BM for intra-band UL CA

 -- R1 22-5c: Simultaneous transmission of SRS for antenna switching and SRS for antenna switching for intra-band UL CA

 simulTX-SRS-AntSwitchingIntraBandUL-CA-r16 SimulSRS-ForAntennaSwitching-r16 OPTIONAL,

 -- R1 10: NR-unlicensed

 sharedSpectrumChAccessParamsPerBand-v1630 SharedSpectrumChAccessParamsPerBand-v1630 OPTIONAL

 ]],

 [[

 handoverUTRA-FDD-r16 ENUMERATED {supported} OPTIONAL,

 -- R4 7-4: Report the shorter transient capability supported by the UE: 2, 4 or 7us

 enhancedUL-TransientPeriod-r16 ENUMERATED {us2, us4, us7} OPTIONAL,

 sharedSpectrumChAccessParamsPerBand-v1640 SharedSpectrumChAccessParamsPerBand-v1640 OPTIONAL

 ]],

 [[

 type1-PUSCH-RepetitionMultiSlots-v1650 ENUMERATED {supported} OPTIONAL,

 type2-PUSCH-RepetitionMultiSlots-v1650 ENUMERATED {supported} OPTIONAL,

 pusch-RepetitionMultiSlots-v1650 ENUMERATED {supported} OPTIONAL,

 configuredUL-GrantType1-v1650 ENUMERATED {supported} OPTIONAL,

 configuredUL-GrantType2-v1650 ENUMERATED {supported} OPTIONAL,

 sharedSpectrumChAccessParamsPerBand-v1650 SharedSpectrumChAccessParamsPerBand-v1650 OPTIONAL

 ]],

 [[

 enhancedSkipUplinkTxConfigured-v1660 ENUMERATED {supported} OPTIONAL,

 enhancedSkipUplinkTxDynamic-v1660 ENUMERATED {supported} OPTIONAL

 ]],

 [[

 maxUplinkDutyCycle-PC1dot5-MPE-FR1-r16 ENUMERATED {n10, n15, n20, n25, n30, n40, n50, n60, n70, n80, n90, n100} OPTIONAL,

 txDiversity-r16 ENUMERATED {supported} OPTIONAL

 ]],

 [[

 -- R1 36-1: Support of 1024QAM for PDSCH for FR1

 pdsch-1024QAM-FR1-r17 ENUMERATED {supported} OPTIONAL,

 -- R4 22-1 support of FR2 HST operation

 ue-PowerClass-v1700 ENUMERATED {pc5, pc6, pc7} OPTIONAL,

 -- R1 24: NR extension to 71GHz (FR2-2)

 fr2-2-AccessParamsPerBand-r17 FR2-2-AccessParamsPerBand-r17 OPTIONAL,

 rlm-Relaxation-r17 ENUMERATED {supported} OPTIONAL,

 bfd-Relaxation-r17 ENUMERATED {supported} OPTIONAL,

 cg-SDT-r17 ENUMERATED {supported} OPTIONAL,

 locationBasedCondHandover-r17 ENUMERATED {supported} OPTIONAL,

 timeBasedCondHandover-r17 ENUMERATED {supported} OPTIONAL,

 eventA4BasedCondHandover-r17 ENUMERATED {supported} OPTIONAL,

 mn-InitiatedCondPSCellChangeNRDC-r17 ENUMERATED {supported} OPTIONAL,

 sn-InitiatedCondPSCellChangeNRDC-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 29-3a: PDCCH skipping

 pdcch-SkippingWithoutSSSG-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 29-3b: 2 search space sets group switching

 sssg-Switching-1BitInd-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 29-3c: 3 search space sets group switching

 sssg-Switching-2BitInd-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 29-3d: 2 search space sets group switching with PDCCH skipping

 pdcch-SkippingWithSSSG-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 29-3e: Support Search space set group switching capability 2 for FR1

 searchSpaceSetGrp-switchCap2-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 26-1: Uplink Time and Frequency pre-compensation and timing relationship enhancements

 uplinkPreCompensation-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 26-4: UE reporting of information related to TA pre-compensation

 uplink-TA-Reporting-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 26-5: Increasing the number of HARQ processes

 max-HARQ-ProcessNumber-r17 ENUMERATED {u16d32, u32d16, u32d32} OPTIONAL,

 -- R1 26-6: Type-2 HARQ codebook enhancement

 type2-HARQ-Codebook-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 26-6a: Type-1 HARQ codebook enhancement

 type1-HARQ-Codebook-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 26-6b: Type-3 HARQ codebook enhancement

 type3-HARQ-Codebook-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 26-9: UE-specific K\_offset

 ue-specific-K-Offset-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 24-1f: Multiple PDSCH scheduling by single DCI for 120kHz in FR2-1

 multiPDSCH-SingleDCI-FR2-1-SCS-120kHz-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 24-1g: Multiple PUSCH scheduling by single DCI for 120kHz in FR2-1

 multiPUSCH-SingleDCI-FR2-1-SCS-120kHz-r17 ENUMERATED {supported} OPTIONAL,

 -- R4 14-4: Parallel PRS measurements in RRC\_INACTIVE state, FR1/FR2 diff

 parallelPRS-MeasRRC-Inactive-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 27-1-2: Support of UE-TxTEGs for UL TDOA

 nr-UE-TxTEG-ID-MaxSupport-r17 ENUMERATED {n1, n2, n3, n4, n6, n8} OPTIONAL,

 -- R1 27-17: PRS processing in RRC\_INACTIVE

 prs-ProcessingRRC-Inactive-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 27-3-2: DL PRS measurement outside MG and in a PRS processing window

 prs-ProcessingWindowType1A-r17 ENUMERATED {option1, option2, option3} OPTIONAL,

 prs-ProcessingWindowType1B-r17 ENUMERATED {option1, option2, option3} OPTIONAL,

 prs-ProcessingWindowType2-r17 ENUMERATED {option1, option2, option3} OPTIONAL,

 -- R1 27-15: Positioning SRS transmission in RRC\_INACTIVE state for initial UL BWP

 srs-AllPosResourcesRRC-Inactive-r17 SRS-AllPosResourcesRRC-Inactive-r17 OPTIONAL,

 -- R1 27-16: OLPC for positioning SRS in RRC\_INACTIVE state - gNB

 olpc-SRS-PosRRC-Inactive-r17 OLPC-SRS-Pos-r16 OPTIONAL,

 -- R1 27-19: Spatial relation for positioning SRS in RRC\_INACTIVE state - gNB

 spatialRelationsSRS-PosRRC-Inactive-r17 SpatialRelationsSRS-Pos-r16 OPTIONAL,

 -- R1 30-1: Increased maximum number of PUSCH Type A repetitions

 maxNumberPUSCH-TypeA-Repetition-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 30-2: PUSCH Type A repetitions based on available slots

 puschTypeA-RepetitionsAvailSlot-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 30-3: TB processing over multi-slot PUSCH

 tb-ProcessingMultiSlotPUSCH-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 30-3a: Repetition of TB processing over multi-slot PUSCH

 tb-ProcessingRepMultiSlotPUSCH-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 30-4: The maximum duration for DM-RS bundling

 maxDurationDMRS-Bundling-r17 SEQUENCE {

 fdd-r17 ENUMERATED {n4, n8, n16, n32} OPTIONAL,

 tdd-r17 ENUMERATED {n2, n4, n8, n16} OPTIONAL

 } OPTIONAL,

 -- R1 30-6: Repetition of PUSCH transmission scheduled by RAR UL grant and DCI format 0\_0 with CRC scrambled by TC-RNTI

 pusch-RepetitionMsg3-r17 ENUMERATED {supported} OPTIONAL,

 sharedSpectrumChAccessParamsPerBand-v1710 SharedSpectrumChAccessParamsPerBand-v1710 OPTIONAL,

 -- R4 25-2: Parallel measurements on cells belonging to a different NGSO satellite than a serving satellite without scheduling restrictions

 -- on normal operations with the serving cell

 parallelMeasurementWithoutRestriction-r17 ENUMERATED {supported} OPTIONAL,

 -- R4 25-5: Parallel measurements on multiple NGSO satellites within a SMTC

 maxNumber-NGSO-SatellitesWithinOneSMTC-r17 ENUMERATED {n1, n2, n3, n4} OPTIONAL,

 -- R1 26-10: K1 range extension

 k1-RangeExtension-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 35-1: Aperiodic CSI-RS for tracking for fast SCell activation

 aperiodicCSI-RS-FastScellActivation-r17 SEQUENCE {

 maxNumberAperiodicCSI-RS-PerCC-r17 ENUMERATED {n8, n16, n32, n48, n64, n128, n255},

 maxNumberAperiodicCSI-RS-AcrossCCs-r17 ENUMERATED {n8, n16, n32, n64, n128, n256, n512, n1024}

 } OPTIONAL,

 -- R1 35-2: Aperiodic CSI-RS bandwidth for tracking for fast SCell activation for 10MHz UE channel bandwidth

 aperiodicCSI-RS-AdditionalBandwidth-r17 ENUMERATED {addBW-Set1, addBW-Set2} OPTIONAL,

 -- R1 28-1a: RRC-configured DL BWP without CD-SSB or NCD-SSB

 bwp-WithoutCD-SSB-OrNCD-SSB-RedCap-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 28-3: Half-duplex FDD operation type A for (e)RedCap UE

 halfDuplexFDD-TypeA-RedCap-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 27-15b: Positioning SRS transmission in RRC\_INACTIVE state configured outside initial UL BWP

 posSRS-RRC-Inactive-OutsideInitialUL-BWP-r17 PosSRS-RRC-Inactive-OutsideInitialUL-BWP-r17 OPTIONAL,

 -- R4 15-3 UE support of CBW for 480kHz SCS

 channelBWs-DL-SCS-480kHz-FR2-2-r17 BIT STRING (SIZE (8)) OPTIONAL,

 channelBWs-UL-SCS-480kHz-FR2-2-r17 BIT STRING (SIZE (8)) OPTIONAL,

 -- R4 15-4 UE support of CBW for 960kHz SCS

 channelBWs-DL-SCS-960kHz-FR2-2-r17 BIT STRING (SIZE (8)) OPTIONAL,

 channelBWs-UL-SCS-960kHz-FR2-2-r17 BIT STRING (SIZE (8)) OPTIONAL,

 -- R4 17-1 UL gap for Tx power management

 ul-GapFR2-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 25-4: One-shot HARQ ACK feedback triggered by DCI format 1\_2

 oneShotHARQ-feedbackTriggeredByDCI-1-2-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 25-5: PHY priority handling for one-shot HARQ ACK feedback

 oneShotHARQ-feedbackPhy-Priority-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 25-6: Enhanced type 3 HARQ-ACK codebook feedback

 enhancedType3-HARQ-CodebookFeedback-r17 SEQUENCE {

 enhancedType3-HARQ-Codebooks-r17 ENUMERATED {n1, n2, n4, n8},

 maxNumberPUCCH-Transmissions-r17 ENUMERATED {n1, n2, n3, n4, n5, n6, n7}

 } OPTIONAL,

 -- R1 25-7: Triggered HARQ-ACK codebook re-transmission

 triggeredHARQ-CodebookRetx-r17 SEQUENCE {

 minHARQ-Retx-Offset-r17 ENUMERATED {n-7, n-5, n-3, n-1, n1},

 maxHARQ-Retx-Offset-r17 ENUMERATED {n4, n6, n8, n10, n12, n14, n16, n18, n20, n22, n24}

 } OPTIONAL

 ]],

 [[

 -- R4 22-2 support of one shot large UL timing adjustment

 ue-OneShotUL-TimingAdj-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 25-2: Repetitions for PUCCH format 0, and 2 over multiple slots with K = 2, 4, 8

 pucch-Repetition-F0-2-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 25-11a: 4-bits subband CQI for NTN and unlicensed

 cqi-4-BitsSubbandNTN-SharedSpectrumChAccess-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 25-16: HARQ-ACK with different priorities multiplexing on a PUCCH/PUSCH

 mux-HARQ-ACK-DiffPriorities-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 25-20a: Propagation delay compensation based on Rel-15 TA procedure for NTN and unlicensed

 ta-BasedPDC-NTN-SharedSpectrumChAccess-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 33-2b: DCI-based enabling/disabling ACK/NACK-based feedback for dynamic scheduling for multicast

 ack-NACK-FeedbackForMulticastWithDCI-Enabler-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 33-2e: Multiple G-RNTIs for group-common PDSCHs

 maxNumberG-RNTI-r17 INTEGER (2..8) OPTIONAL,

 -- R1 33-2f: Dynamic multicast with DCI format 4\_2

 dynamicMulticastDCI-Format4-2-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 33-2i: Supported maximal modulation order for multicast PDSCH

 maxModulationOrderForMulticast-r17 CHOICE {

 fr1-r17 ENUMERATED {qam256, qam1024},

 fr2-r17 ENUMERATED {qam64, qam256}

 } OPTIONAL,

 -- R1 33-3-1: Dynamic Slot-level repetition for group-common PDSCH for TN and licensed

 dynamicSlotRepetitionMulticastTN-NonSharedSpectrumChAccess-r17 ENUMERATED {n8, n16} OPTIONAL,

 -- R1 33-3-1a: Dynamic Slot-level repetition for group-common PDSCH for NTN and unlicensed

 dynamicSlotRepetitionMulticastNTN-SharedSpectrumChAccess-r17 ENUMERATED {n8, n16} OPTIONAL,

 -- R1 33-4-1: DCI-based enabling/disabling NACK-only based feedback for dynamic scheduling for multicast

 nack-OnlyFeedbackForMulticastWithDCI-Enabler-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 33-5-1b: DCI-based enabling/disabling ACK/NACK-based feedback for dynamic scheduling for multicast

 ack-NACK-FeedbackForSPS-MulticastWithDCI-Enabler-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 33-5-1h: Multiple G-CS-RNTIs for SPS group-common PDSCHs

 maxNumberG-CS-RNTI-r17 INTEGER (2..8) OPTIONAL,

 -- R1 33-10: Support group-common PDSCH RE-level rate matching for multicast

 re-LevelRateMatchingForMulticast-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 36-1a: Support of 1024QAM for PDSCH with maximum 2 MIMO layers for FR1

 pdsch-1024QAM-2MIMO-FR1-r17 ENUMERATED {supported} OPTIONAL,

 -- R4 14-3 PRS measurement without MG

 prs-MeasurementWithoutMG-r17 ENUMERATED {cpLength, quarterSymbol, halfSymbol, halfSlot} OPTIONAL,

 -- R4 25-7: The number of target LEO satellites the UE can monitor per carrier

 maxNumber-LEO-SatellitesPerCarrier-r17 INTEGER (3..4) OPTIONAL,

 -- R1 27-3-3 DL PRS Processing Capability outside MG - buffering capability

 prs-ProcessingCapabilityOutsideMGinPPW-r17 SEQUENCE (SIZE(1..3)) OF PRS-ProcessingCapabilityOutsideMGinPPWperType-r17 OPTIONAL,

 -- R1 27-15a: Positioning SRS transmission in RRC\_INACTIVE state for initial UL BWP with semi-persistent SRS

 srs-SemiPersistent-PosResourcesRRC-Inactive-r17 SEQUENCE {

 maxNumOfSemiPersistentSRSposResources-r17 ENUMERATED {n1, n2, n4, n8, n16, n32, n64},

 maxNumOfSemiPersistentSRSposResourcesPerSlot-r17 ENUMERATED {n1, n2, n3, n4, n5, n6, n8, n10, n12, n14}

 } OPTIONAL,

 -- R2: UE support of CBW for 120kHz SCS

 channelBWs-DL-SCS-120kHz-FR2-2-r17 BIT STRING (SIZE (8)) OPTIONAL,

 channelBWs-UL-SCS-120kHz-FR2-2-r17 BIT STRING (SIZE (8)) OPTIONAL

 ]],

 [[

 -- R1 30-4a: DM-RS bundling for PUSCH repetition type A

 dmrs-BundlingPUSCH-RepTypeA-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 30-4b: DM-RS bundling for PUSCH repetition type B

 dmrs-BundlingPUSCH-RepTypeB-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 30-4c: DM-RS bundling for TB processing over multi-slot PUSCH

 dmrs-BundlingPUSCH-multiSlot-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 30-4d: DMRS bundling for PUCCH repetitions

 dmrs-BundlingPUCCH-Rep-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 30-4e: Enhanced inter-slot frequency hopping with inter-slot bundling for PUSCH

 interSlotFreqHopInterSlotBundlingPUSCH-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 30-4f: Enhanced inter-slot frequency hopping for PUCCH repetitions with DMRS bundling

 interSlotFreqHopPUCCH-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 30-4g: Restart DM-RS bundling

 dmrs-BundlingRestart-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 30-4h: DM-RS bundling for non-back-to-back transmission

 dmrs-BundlingNonBackToBackTX-r17 ENUMERATED {supported} OPTIONAL

 ]],

 [[

 -- R1 33-5-1e: Dynamic Slot-level repetition for SPS group-common PDSCH for multicast

 maxDynamicSlotRepetitionForSPS-Multicast-r17 ENUMERATED {n8, n16} OPTIONAL,

 -- R1 33-5-1g: DCI-based enabling/disabling NACK-only based feedback for SPS group-common PDSCH for multicast

 nack-OnlyFeedbackForSPS-MulticastWithDCI-Enabler-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 33-5-1i: Multicast SPS scheduling with DCI format 4\_2

 sps-MulticastDCI-Format4-2-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 33-5-2: Multiple SPS group-common PDSCH configuration on PCell

 sps-MulticastMultiConfig-r17 INTEGER (1..8) OPTIONAL,

 -- R1 33-6-1: DL priority indication for multicast in DCI

 priorityIndicatorInDCI-Multicast-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 33-6-1a: DL priority configuration for SPS multicast

 priorityIndicatorInDCI-SPS-Multicast-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 33-6-2: Two HARQ-ACK codebooks simultaneously constructed for supporting HARQ-ACK codebooks with different priorities

 -- for unicast and multicast at a UE

 twoHARQ-ACK-CodebookForUnicastAndMulticast-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 33-6-3: More than one PUCCH for HARQ-ACK transmission for multicast or for unicast and multicast within a slot

 multiPUCCH-HARQ-ACK-ForMulticastUnicast-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 33-9: Supporting unicast PDCCH to release SPS group-common PDSCH

 releaseSPS-MulticastWithCS-RNTI-r17 ENUMERATED {supported} OPTIONAL

 ]],

 [[

 -- R1 41-3-1a UE automomous TA adjustment when cell-reselection happens

 posUE-TA-AutoAdjustment-r18 ENUMERATED {supported} OPTIONAL,

 -- R1 41-4-6a support a Rel-17 single DCI scheduling positioning SRS resource sets across the linked carriers

 -- for SRS bandwidth aggregation in RRC\_CONNECTED state

 posJointTriggerBySingleDCI-RRC-Connected-r18 ENUMERATED {supported} OPTIONAL,

 -- R1 41-5-1a PRS measurement with Rx frequency hopping in RRC\_INACTIVE for RedCap UEs

 dl-PRS-MeasurementWithRxFH-RRC-InactiveforRedCap-r18 ENUMERATED {supported} OPTIONAL,

 -- R1 41-5-1b PRS measurement with Rx frequency hopping in RRC\_IDLE for RedCap UEs

 dl-PRS-MeasurementWithRxFH-RRC-IdleforRedCap-r18 ENUMERATED {supported} OPTIONAL,

 -- R1 42-4: Cell DTX and/or DRX operation based on RRC configuration

 nes-CellDTX-DRX-r18 ENUMERATED {cellDTXonly, cellDRXonly, both} OPTIONAL,

 -- R1 42-5: Cell DTX/DRX operation triggered by DCI format 2\_9

 nes-CellDTX-DRX-DCI2-9-r18 ENUMERATED {supported} OPTIONAL,

 -- R1 45-6: UE-based TA measurement

 ue-TA-Measurement-r18 INTEGER (1..8) OPTIONAL,

 -- R1 45-7: TA indication in cell switch command

 ta-IndicationCellSwitch-r18 ENUMERATED {supported} OPTIONAL,

 -- R1 50-1: Multi-PUSCHs for Configured Grant

 multiPUSCH-CG-r18 ENUMERATED {n16, n32} OPTIONAL,

 -- R1 50-1a: Multiple active multi-PUSCHs configured grant configurations for a BWP of a serving cell

 multiPUSCH-ActiveConfiguredGrant-r18 SEQUENCE {

 maxNumberConfigsPerBWP ENUMERATED {n1, n2, n4, n8, n12},

 maxNumberConfigsAllCC-FR1 INTEGER (2..32),

 maxNumberConfigsAllCC-FR2 INTEGER (2..32)

 } OPTIONAL,

 -- R1 50-2: UCI indication of unused CG-PUSCH transmission occasions

 cg-PUSCH-UTO-UCI-Ind-r18 ENUMERATED {supported} OPTIONAL,

 -- R1 50-3: PDCCH monitoring resumption after UL NACK

 pdcch-MonitoringResumptionAfterUL-NACK-r18 ENUMERATED {supported} OPTIONAL,

 -- R1 51-1: support for 3MHz channel bandwidth

 support-3MHz-ChannelBW-r18 ENUMERATED {supported} OPTIONAL,

 -- R1 51-2: support 12 PRB CORESET0

 support-12PRB-CORESET0-r18 ENUMERATED {supported} OPTIONAL,

 -- R1 52-1: Reception of NR PDCCH candidates overlapping with LTE CRS REs

 nr-PDCCH-OverlapLTE-CRS-RE-r18 SEQUENCE {

 overlapInRE-r18 ENUMERATED {oneSymbolNoOverlap, someOrAllSymOverlap},

 overlapInSymbol-r18 ENUMERATED {symbol2,symbol1And2}

 } OPTIONAL,

 -- Editor's Note: someOrAllSymOverlap considers to be supported in overlapInRE-r18 only if RAN4 performance requirements for

 -- someOrAllSymOverlap are not defined

 -- R1 52-1a: Reception of NR PDCCH candidates overlapping with LTE CRS REs with multiple non-overlapping CRS rate matching patterns

 nr-PDCCH-OverlapLTE-CRS-RE-MultiPatterns-r18 ENUMERATED {supported} OPTIONAL,

 -- R1 52-1b: NR PDCCH reception that overlaps with LTE CRS within a single span of 3 consecutive OFDM symbols that is within the

 -- first 4 OFDM symbols in a slot

 nr-PDCCH-OverlapLTE-CRS-RE-Span-3-4-r18 ENUMERATED {supported} OPTIONAL,

 -- R1 52-2: Two LTE-CRS overlapping rate matching patterns within NR 15 kHz carrier overlapping with LTE carrier (regardless of

 -- support or configuration of multi-TRP)

 twoRateMatchingEUTRA-CRS-patterns-3-4-r18 SEQUENCE {

 maxNumberPatterns-r18 INTEGER (2..6),

 maxNumberNon-OverlapPatterns-r18 INTEGER (1..3)

 } OPTIONAL,

 -- R1 52-2a: Two LTE-CRS overlapping rate matching patterns with two different values of coresetPoolIndex within NR 15 kHz carrier

 -- overlapping with LTE carrier

 overlapRateMatchingEUTRA-CRS-Patterns-3-4-Diff-CS-Pool-r18 ENUMERATED {supported} OPTIONAL,

 -- R1 53-3: Support RLM/BM/BFD measurements based on NCD-SSB within active BWP

 ncd-SSB-BWP-Wor-r18 ENUMERATED {supported} OPTIONAL,

 -- R1 53-4: Support Support RLM/BM/BFD measurements based on CSI-RS when CD-SSB is outside active BWP

 rlm-BM-BFD-CSI-RS-OutsideActiveBWP-r18 ENUMERATED {supported} OPTIONAL,

 -- R1 55-3: Multiple PUSCHs scheduling by single DCI for non-consecutive slots in FR1

 multiPUSCH-SingleDCI-NonConsSlots-r18 ENUMERATED {supported} OPTIONAL,

 -- R1 55-2d: single-symbol DL-PRS used in RTT-based Propagation delay compensation

 pdc-maxNumberPRS-ResourceProcessedPerSlot-r18 SEQUENCE {

 fr1-r18 SEQUENCE {

 scs-15kHz-r18 ENUMERATED {n1, n2, n4, n6, n8, n12, n16, n24, n32, n48, n64} OPTIONAL,

 scs-30kHz-r18 ENUMERATED {n1, n2, n4, n6, n8, n12, n16, n24, n32, n48, n64} OPTIONAL,

 scs-60kHz-r18 ENUMERATED {n1, n2, n4, n6, n8, n12, n16, n24, n32, n48, n64} OPTIONAL

 },

 fr2-r18 SEQUENCE {

 scs-60kHz-r18 ENUMERATED {n1, n2, n4, n6, n8, n12, n16, n24, n32, n48, n64} OPTIONAL,

 scs-120kHz-r18 ENUMERATED {n1, n2, n4, n6, n8, n12, n16, n24, n32, n48, n64} OPTIONAL

 }

 } OPTIONAL,

 -- R4 27-2: LowerMSD for inter-band NR CA and EN-DC

 lowerMSD-r18 SEQUENCE (SIZE (1..maxLowerMSD-r18)) OF LowerMSD-r18 OPTIONAL,

 -- R4 31-2 Beam sweeping factor reduction for FR2 unknown SCell activation

 beamSweepingFactorReduction-r18 SEQUENCE {

 reduceForCellDetection ENUMERATED {n1, n2, n4, n6},

 reduceForSSB-L1-RSRP-Meas INTEGER (0..7)

 } OPTIONAL,

 -- R4 35-2: the requirements defined for ATG UE with antenna array or omni-direction antenna requirements.

 antennaArrayType-r18 ENUMERATED {supported} OPTIONAL,

 locationBasedCondHandoverATG-r18 ENUMERATED {supported} OPTIONAL,

 -- R4 35-3: rated maximum output power value range from 23dBm to 40dBm with 1dB as granularity at maximum modulation order and full

 -- PRB configurations.

 maxOutputPowerATG-r18 INTEGER (1..18) OPTIONAL,

 eventA4BasedCondHandoverNES-r18 ENUMERATED {supported} OPTIONAL,

 nesBasedCondHandoverWithDCI-r18 ENUMERATED {supported} OPTIONAL,

 rachLessHandoverNTN-r18 ENUMERATED {supported} OPTIONAL,

 locationBasedCondHandoverEMC-r18 ENUMERATED {supported} OPTIONAL,

 mt-CG-SDT-r18 ENUMERATED {supported} OPTIONAL,

 posSRS-RRC-InactiveInitialUL-BWP-r18 ENUMERATED {supported} OPTIONAL,

 posSRS-RRC-InactiveOutsideInitialUL-BWP-r18 ENUMERATED {supported} OPTIONAL,

 cg-SDT-PeriodicityExt-r18 ENUMERATED {supported} OPTIONAL,

 -- R2: 2Rx XR UEs

 supportOf2RxXR-r18 ENUMERATED {supported} OPTIONAL

 ]]

}

BandNR-v16c0 ::= SEQUENCE {

 pusch-RepetitionTypeA-v16c0 ENUMERATED {supported} OPTIONAL,

 ...

}

LowerMSD-r18 ::= SEQUENCE {

 aggressorband1-r18 FreqBandIndicatorNR,

 aggressorband2-r18 FreqBandIndicatorNR OPTIONAL,

 msd-Information-r18 SEQUENCE (SIZE (1..maxLowerMSDInfo-r18)) OF MSD-Information-r18

}

MSD-Information-r18 ::= SEQUENCE {

 msd-Type-r18 ENUMERATED {harmonic, harmonicMixing, crossBandIsolation, imd2, imd3, imd4, imd5, all, spare8, spare7,

 spare6, spare5,spare4, spare3, spare2, spare1},

 msd-PowerClass-r18 ENUMERATED {pc1dot5, pc2, pc3},

 msd-Class-r18 ENUMERATED {classI, classII, classIII, classIV, classV, classVI, classVII, classVIII }

}

-- Editor note: The power class related part can be updated further pending RAN4 discussion.

-- TAG-RF-PARAMETERS-STOP

-- ASN1STOP

|  |
| --- |
| *RF-Parameters* field descriptions |
| ***appliedFreqBandListFilter***In this field the UE mirrors the *FreqBandList* that the NW provided in the capability enquiry, if any, as described in clause 5.6.1.4. The UE filtered the band combinations in the *supportedBandCombinationList* in accordance with this *appliedFreqBandListFilter*. The UE does not include this field if the UE capability is requested by E-UTRAN and the network request includes the field *eutra-nr-only* [10]. |
| ***supportedBandCombinationList***A list of band combinations that the UE supports for NR (and NR-DC, if requested). The *FeatureSetCombinationId*:s in this list refer to the *FeatureSetCombination* entries in the *featureSetCombinations* list in the *UE-NR-Capability* IE. The UE does not include this field if the UE capability is requested by E-UTRAN and the network request includes the field *eutra-nr-only* [10]. |
| ***supportedBandCombinationListSidelinkEUTRA-NR***A list of band combinations that the UE supports for NR sidelink communication only, for joint NR sidelink communication and V2X sidelink communication, or for V2X sidelink communication only. The UE does not include this field if the UE capability is requested by E-UTRAN (see TS 36.331[10]) and the network request includes the field *eutra-nr-only*. |
| ***supportedBandCombinationListSL-NonRelayDiscovery***A list of band combinations that the UE supports for NR sidelink non-relay discovery. The encoding is defined in PC5 *BandCombinationListSidelinkNR-r16.* |
| ***supportedBandCombinationListSL-RelayDiscovery***A list of band combinations that the UE supports for NR sidelink relay discovery. The encoding is defined in PC5 *BandCombinationListSidelinkNR-r16.* |
| ***supportedBandCombinationListSL-U2U-DiscoveryExt***This field indicates the band parameter in *BandCombinationListSL-Discovery-r17* that the UE supports for NR U2U sidelink relay discovery in a band included in *supportedBandCombinationListSL-U2U-RelayDiscovery*. |
| ***supportedBandCombinationListSL-U2U-RelayDiscovery***A list of band combinations that the UE supports for NR U2U sidelink relay discovery. The encoding is defined in PC5 *BandCombinationListSidelinkNR-r16.* |
| ***supportedBandCombinationList-UplinkTxSwitch***A list of band combinations that the UE supports dynamic uplink Tx switching for NR UL CA and SUL. The *FeatureSetCombinationId*:s in this list refer to the *FeatureSetCombination* entries in the *featureSetCombinations* list in the *UE-NR-Capability* IE. The UE does not include this field if the UE capability is requested by E-UTRAN and the network request includes the field *eutra-nr-only* [10]. |
| ***supportedBandListNR***A list of NR bands supported by the UE. If *supportedBandListNR-v16c0* is included, the UE shall include the same number of entries, and listed in the same order, as in *supportedBandListNR* (without suffix). |

### 11.2.2 Message definitions

#### – *UERadioPagingInformation*

This message is used to transfer radio paging information, covering both upload to and download from the 5GC, and between gNBs.

Direction: gNB to/ from 5GC and gNB to/from gNB

*UERadioPagingInformation* message

-- ASN1START

-- TAG-UE-RADIO-PAGING-INFORMATION-START

UERadioPagingInformation ::= SEQUENCE {

 criticalExtensions CHOICE {

 c1 CHOICE{

 ueRadioPagingInformation UERadioPagingInformation-IEs,

 spare7 NULL,

 spare6 NULL, spare5 NULL, spare4 NULL,

 spare3 NULL, spare2 NULL, spare1 NULL

 },

 criticalExtensionsFuture SEQUENCE {}

 }

}

UERadioPagingInformation-IEs ::= SEQUENCE {

 supportedBandListNRForPaging SEQUENCE (SIZE (1..maxBands)) OF FreqBandIndicatorNR OPTIONAL,

 nonCriticalExtension UERadioPagingInformation-v15e0-IEs OPTIONAL

}

UERadioPagingInformation-v15e0-IEs ::= SEQUENCE {

 dl-SchedulingOffset-PDSCH-TypeA-FDD-FR1 ENUMERATED {supported} OPTIONAL,

 dl-SchedulingOffset-PDSCH-TypeA-TDD-FR1 ENUMERATED {supported} OPTIONAL,

 dl-SchedulingOffset-PDSCH-TypeA-TDD-FR2 ENUMERATED {supported} OPTIONAL,

 dl-SchedulingOffset-PDSCH-TypeB-FDD-FR1 ENUMERATED {supported} OPTIONAL,

 dl-SchedulingOffset-PDSCH-TypeB-TDD-FR1 ENUMERATED {supported} OPTIONAL,

 dl-SchedulingOffset-PDSCH-TypeB-TDD-FR2 ENUMERATED {supported} OPTIONAL,

 nonCriticalExtension UERadioPagingInformation-v1700-IEs OPTIONAL

}

UERadioPagingInformation-v1700-IEs ::= SEQUENCE {

 ue-RadioPagingInfo-r17 OCTET STRING (CONTAINING UE-RadioPagingInfo-r17) OPTIONAL,

 inactiveStatePO-Determination-r17 ENUMERATED {supported} OPTIONAL,

 numberOfRxRedCap-r17 ENUMERATED {one, two} OPTIONAL,

 halfDuplexFDD-TypeA-RedCap-r17 SEQUENCE (SIZE (1..maxBands)) OF FreqBandIndicatorNR OPTIONAL,

 nonCriticalExtension UERadioPagingInformation-v1800-IEs OPTIONAL

}

UERadioPagingInformation-v1800-IEs ::= SEQUENCE {

 numberOfRxERedCap-r18 ENUMERATED {one, two} OPTIONAL,

 supportOf2RxXR-r18 ENUMERATED {supported} OPTIONAL,

 nonCriticalExtension SEQUENCE {} OPTIONAL

}

-- TAG-UE-RADIO-PAGING-INFORMATION-STOP

-- ASN1STOP

| *UERadioPagingInformation* field descriptions |
| --- |
| ***supportedBandListNRForPaging***Indicates the UE supported NR frequency bands which are derived by the gNB from *UE-NR-Capability*. |
| ***dl-SchedulingOffset-PDSCH-TypeA-FDD-FR1***Indicates whether the UE supports DL scheduling slot offset (K0) greater than 0 for PDSCH mapping type A in FDD FR1. |
| ***dl-SchedulingOffset-PDSCH-TypeA-TDD-FR1***Indicates whether the UE supports DL scheduling slot offset (K0) greater than 0 for PDSCH mapping type A in TDD FR1. |
| ***dl-SchedulingOffset-PDSCH-TypeA-TDD-FR2***Indicates whether the UE supports DL scheduling slot offset (K0) greater than 0 for PDSCH mapping type A in TDD FR2. |
| ***dl-SchedulingOffset-PDSCH-TypeB-FDD-FR1***Indicates whether the UE supports DL scheduling slot offset (K0) greater than 0 for PDSCH mapping type B in FDD FR1. |
| ***dl-SchedulingOffset-PDSCH-TypeB-TDD-FR1***Indicates whether the UE supports DL scheduling slot offset (K0) greater than 0 for PDSCH mapping type B in TDD FR1. |
| ***dl-SchedulingOffset-PDSCH-TypeB-TDD-FR2***Indicates whether the UE supports DL scheduling slot offset (K0) greater than 0 for PDSCH mapping type B in TDD FR2. |
| ***halfDuplexFDD-TypeA-RedCap***Indicates whether the (e)RedCap UE only supports half-duplex operation for FDD in the indicated band(s). |
| ***inactiveStatePO-Determination***Indicates whether the UE supports to use the same i\_s to determine PO in RRC\_INACTIVE state as in RRC\_IDLE state. |
| ***numberOfRxERedCap***Indicates the number of Rx branches supported by an eRedCap UE. |
| ***numberOfRxRedCap***Indicates the number of Rx branches supported by a RedCap UE. |
| ***supportOf2RxXR***Indicates whether the UE is a 2Rx XR UE.  |
| ***ue-RadioPagingInfo***The field is used to transfer UE capability information used for paging. The gNB generates the ue-RadioPagingInfo and the contained UE capability information is absent when not supported by the UE. |