|  |  |  |
| --- | --- | --- |
| **Company** | **Clause Number and Related specification** | **Comment** |
| Xiaomi | 5.8.9.1a.4  Do we need to reflect the condition for RRC\_IDLE/INACTIVE when duplication is configured and for all RRC states when duplication is not configured？ |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |