|  |  |  |
| --- | --- | --- |
| **Company** | **Clause Number and Related specification** | **Comment** |
| Xiaomi | 5.8.9.1a.4  Do we need to reflect the condition for RRC\_IDLE/INACTIVE when duplication is configured and for all RRC states when duplication is not configured？ | [Rapp] after offline with Xiaomi, I understand the key point is about how to understand the case that “RRC\_CONNECTED UE with duplication is configured”, for which network will provide two carrier sets explicitly. But it seems better to further discuss/clarify this issue a bit more before reflecting it in spec. So suggest to pend this change till next meeting. |
| Huawei, HiSilicon | The agreed changes based on P2, P3 in R2-2402227 are added in the section for PC5-S message:  1> if transmission of PC5-S message for a specific destination is requested by upper layers for sidelink SRB:  Should be added instead in the section for PC5-RRC message (?):  1> if a PC5-RRC connection establishment for a specific destination is indicated by upper layers: | [Rapp] Agree with the point that this conclusion also applies to PC5-RRC, yet it should be also applicable to PC5-S? not sure if I misunderstood any point here? If so, please be free to correct, thanks!  [Huawei, HiSilicon] Regarding PC5-S carriers, our understanding is that SA2 has yet to finalized on the conclusion "whether the upper layer indicates the carriers for the PC5-S messages". If SA2 finally decides the higher layer indicates carriers for PC5-S message, the section under "1> if transmission of PC5-S message for a specific destination is requested by upper layers for sidelink SRB:" needs to be corrected. With indicated carrier from the upper layer, there is no point for the UE to derive the "superset". On the other hand, if SA2 finally has not conclusion on this matter, we are open to keep the current texts for PC5-S messages. |
| Huawei, HiSilicon | 6.3.5, for Type " SL-Unlicensed-r18 " under IE "SL-BWP-Config", there is one type: contigousRB-> contiguousRB |  |
|  |  |  |