**3GPP TSG-RAN WG2 Meeting #126 R2-24XXXXX**

**Fukuoka, Japan, 20th May– 24th May, 2024**

|  |
| --- |
| *CR-Form-v12.3* |
| **CHANGE REQUEST** |
|  |
|  | **38.331** | **CR** | **draft** | **rev** | **-** | **Current version:** | **18.1.0** |  |
|  |
| *For* ***[HE](http://www.3gpp.org/3G_Specs/CRs.htm%22%20%5Cl%20%22_blank)******[LP](http://www.3gpp.org/3G_Specs/CRs.htm%22%20%5Cl%20%22_blank)*** *on using this form: comprehensive instructions can be found at* *<http://www.3gpp.org/Change-Requests>.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **x** | Radio Access Network | **x** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Correction on NES UE capabilities to 38331 |
|  |  |
| ***Source to WG:*** | vivo |
| ***Source to TSG:*** | RAN2 |
|  |  |
| ***Work item code:*** | Netw\_Energy\_NR-Core |  | ***Date:*** | 2024-05-31 |
|  |  |  |  |  |
| ***Category:*** | F |  | ***Release:*** | Rel-18 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:**Rel-8 (Release 8)**Rel-9 (Release 9)**Rel-10 (Release 10)**Rel-11 (Release 11)**…**Rel-17 (Release 17)**Rel-18 (Release 18)**Rel-19 (Release 19)* *Rel-20 (Release 20)* |
|  |  |
| ***Reason for change:*** | 1. The current field description of *scellWithoutSSB-InterBandCA-r18*does not support the NW to configure CA of a higher-order BC while only configuring inter-band SSB-less operation of a lower-order BC;2. The current field description of *scellWithoutSSB-InterBandCA-r18*does not support the report of multiple inter-band SSB-less SCell operation groups |
|  |  |
| ***Summary of change:*** | Revise the field description of *scellWithoutSSB-InterBandCA-r18* according to the agreements and compromised solution at R2#126:

|  |
| --- |
| Agreements1. Instead of reporting ‘supported’ for a band within the BC to indicate this band can be configured as the reference band for all other bands within the BC, the UE optionally reports ‘referenceBand’ or ‘scellWithoutSSB’ for a band to indicate the support of inter-band SSB-less SCell operation.2. The band indicated as ‘referenceBand’ can be configured as the reference band for all other band(s) indicated as ‘scellWithoutSSB’.3. If the field scellWithoutSSB-InterBandCA-r18 is absent for a band, this band is not involved in the inter-band SSB-less SCell operation.4. If inter-band SSB-less SCell operation is supported between two bands, it is understood that there is no direction between the two bands, which means that the network can configure either band as the reference band and the other band as the SSB-less band.After CB **Compromise solution. CR to be agreed by email** If scheme1 (to be named) is indicated, the band indicated as ‘scheme1’ can be configured as either the reference band or SSB-less band.If scheme2 (to be named) is indicated, the band indicated as ‘referenceBand1’ can be configured as the reference band for all other band(s) indicated as ‘scellWithoutSSB1’, and the band indicated as ‘referenceBand2’ can be configured as the reference band for all other band(s) indicated as ‘scellWithoutSSB2’.If the field scellWithoutSSB-InterBandCA-r18 is absent for a band, this band is not involved in the inter-band SSB-less SCell operation.In a band combination, only scheme1 or scheme2 is indicated. |

 |
|  |  |
| ***Consequences if not approved:*** | Rel-18 NES UE capabilities for supporting inter-band SSB-less SCell operation is limited to the case where all the bands within a BC are involved in the inter-band SSB-less SCell operation and in the same operation group. |
|  |  |
| ***Clauses affected:*** | 6.3.3 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** | **x** |  |  Other core specifications  | TS/TR 38.306 CR ...  |
| ***affected:*** |  | **x** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **x** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

**START OF THE CHANGE**

– *FeatureSetDownlink*

The IE *FeatureSetDownlink* indicates a set of features that the UE supports on the carriers corresponding to one band entry in a band combination.

***FeatureSetDownlink* information element**

-- ASN1START

-- TAG-FEATURESETDOWNLINK-START

FeatureSetDownlink ::= SEQUENCE {

 featureSetListPerDownlinkCC SEQUENCE (SIZE (1..maxNrofServingCells)) OF FeatureSetDownlinkPerCC-Id,

 intraBandFreqSeparationDL FreqSeparationClass OPTIONAL,

 scalingFactor ENUMERATED {f0p4, f0p75, f0p8} OPTIONAL,

 dummy8 ENUMERATED {supported} OPTIONAL,

 scellWithoutSSB ENUMERATED {supported} OPTIONAL,

 csi-RS-MeasSCellWithoutSSB ENUMERATED {supported} OPTIONAL,

 dummy1 ENUMERATED {supported} OPTIONAL,

 type1-3-CSS ENUMERATED {supported} OPTIONAL,

 pdcch-MonitoringAnyOccasions ENUMERATED {withoutDCI-Gap, withDCI-Gap} OPTIONAL,

 dummy2 ENUMERATED {supported} OPTIONAL,

 ue-SpecificUL-DL-Assignment ENUMERATED {supported} OPTIONAL,

 searchSpaceSharingCA-DL ENUMERATED {supported} OPTIONAL,

 timeDurationForQCL SEQUENCE {

 scs-60kHz ENUMERATED {s7, s14, s28} OPTIONAL,

 scs-120kHz ENUMERATED {s14, s28} OPTIONAL

 } OPTIONAL,

 pdsch-ProcessingType1-DifferentTB-PerSlot SEQUENCE {

 scs-15kHz ENUMERATED {upto2, upto4, upto7} OPTIONAL,

 scs-30kHz ENUMERATED {upto2, upto4, upto7} OPTIONAL,

 scs-60kHz ENUMERATED {upto2, upto4, upto7} OPTIONAL,

 scs-120kHz ENUMERATED {upto2, upto4, upto7} OPTIONAL

 } OPTIONAL,

 dummy3 DummyA OPTIONAL,

 dummy4 SEQUENCE (SIZE (1.. maxNrofCodebooks)) OF DummyB OPTIONAL,

 dummy5 SEQUENCE (SIZE (1.. maxNrofCodebooks)) OF DummyC OPTIONAL,

 dummy6 SEQUENCE (SIZE (1.. maxNrofCodebooks)) OF DummyD OPTIONAL,

 dummy7 SEQUENCE (SIZE (1.. maxNrofCodebooks)) OF DummyE OPTIONAL

}

FeatureSetDownlink-v1540 ::= SEQUENCE {

 oneFL-DMRS-TwoAdditionalDMRS-DL ENUMERATED {supported} OPTIONAL,

 additionalDMRS-DL-Alt ENUMERATED {supported} OPTIONAL,

 twoFL-DMRS-TwoAdditionalDMRS-DL ENUMERATED {supported} OPTIONAL,

 oneFL-DMRS-ThreeAdditionalDMRS-DL ENUMERATED {supported} OPTIONAL,

 pdcch-MonitoringAnyOccasionsWithSpanGap SEQUENCE {

 scs-15kHz ENUMERATED {set1, set2, set3} OPTIONAL,

 scs-30kHz ENUMERATED {set1, set2, set3} OPTIONAL,

 scs-60kHz ENUMERATED {set1, set2, set3} OPTIONAL,

 scs-120kHz ENUMERATED {set1, set2, set3} OPTIONAL

 } OPTIONAL,

 pdsch-SeparationWithGap ENUMERATED {supported} OPTIONAL,

 pdsch-ProcessingType2 SEQUENCE {

 scs-15kHz ProcessingParameters OPTIONAL,

 scs-30kHz ProcessingParameters OPTIONAL,

 scs-60kHz ProcessingParameters OPTIONAL

 } OPTIONAL,

 pdsch-ProcessingType2-Limited SEQUENCE {

 differentTB-PerSlot-SCS-30kHz ENUMERATED {upto1, upto2, upto4, upto7}

 } OPTIONAL,

 dl-MCS-TableAlt-DynamicIndication ENUMERATED {supported} OPTIONAL

}

FeatureSetDownlink-v15a0 ::= SEQUENCE {

 supportedSRS-Resources SRS-Resources OPTIONAL

}

FeatureSetDownlink-v1610 ::= SEQUENCE {

 -- R1 22-4e/4f/4g/4h: CBG based reception for DL with unicast PDSCH(s) per slot per CC with UE processing time Capability 1

 cbgPDSCH-ProcessingType1-DifferentTB-PerSlot-r16 SEQUENCE {

 scs-15kHz-r16 ENUMERATED {one, upto2, upto4, upto7} OPTIONAL,

 scs-30kHz-r16 ENUMERATED {one, upto2, upto4, upto7} OPTIONAL,

 scs-60kHz-r16 ENUMERATED {one, upto2, upto4, upto7} OPTIONAL,

 scs-120kHz-r16 ENUMERATED {one, upto2, upto4, upto7} OPTIONAL

 } OPTIONAL,

 -- R1 22-3e/3f/3g/3h: CBG based reception for DL with unicast PDSCH(s) per slot per CC with UE processing time Capability 2

 cbgPDSCH-ProcessingType2-DifferentTB-PerSlot-r16 SEQUENCE {

 scs-15kHz-r16 ENUMERATED {one, upto2, upto4, upto7} OPTIONAL,

 scs-30kHz-r16 ENUMERATED {one, upto2, upto4, upto7} OPTIONAL,

 scs-60kHz-r16 ENUMERATED {one, upto2, upto4, upto7} OPTIONAL,

 scs-120kHz-r16 ENUMERATED {one, upto2, upto4, upto7} OPTIONAL

 } OPTIONAL,

 intraFreqDAPS-r16 SEQUENCE {

 intraFreqDiffSCS-DAPS-r16 ENUMERATED {supported} OPTIONAL,

 intraFreqAsyncDAPS-r16 ENUMERATED {supported} OPTIONAL

 } OPTIONAL,

 intraBandFreqSeparationDL-v1620 FreqSeparationClassDL-v1620 OPTIONAL,

 intraBandFreqSeparationDL-Only-r16 FreqSeparationClassDL-Only-r16 OPTIONAL,

 -- R1 11-2: Rel-16 PDCCH monitoring capability

 pdcch-Monitoring-r16 SEQUENCE {

 pdsch-ProcessingType1-r16 SEQUENCE {

 scs-15kHz-r16 PDCCH-MonitoringOccasions-r16 OPTIONAL,

 scs-30kHz-r16 PDCCH-MonitoringOccasions-r16 OPTIONAL

 } OPTIONAL,

 pdsch-ProcessingType2-r16 SEQUENCE {

 scs-15kHz-r16 PDCCH-MonitoringOccasions-r16 OPTIONAL,

 scs-30kHz-r16 PDCCH-MonitoringOccasions-r16 OPTIONAL

 } OPTIONAL

 } OPTIONAL,

 -- R1 11-2b: Mix of Rel. 16 PDCCH monitoring capability and Rel. 15 PDCCH monitoring capability on different carriers

 pdcch-MonitoringMixed-r16 ENUMERATED {supported} OPTIONAL,

 -- R1 18-5c: Processing up to X unicast DCI scheduling for DL per scheduled CC

 crossCarrierSchedulingProcessing-DiffSCS-r16 SEQUENCE {

 scs-15kHz-120kHz-r16 ENUMERATED {n1,n2,n4} OPTIONAL,

 scs-15kHz-60kHz-r16 ENUMERATED {n1,n2,n4} OPTIONAL,

 scs-30kHz-120kHz-r16 ENUMERATED {n1,n2,n4} OPTIONAL,

 scs-15kHz-30kHz-r16 ENUMERATED {n2} OPTIONAL,

 scs-30kHz-60kHz-r16 ENUMERATED {n2} OPTIONAL,

 scs-60kHz-120kHz-r16 ENUMERATED {n2} OPTIONAL

 } OPTIONAL,

 -- R1 16-2b-1: Support of single-DCI based SDM scheme

 singleDCI-SDM-scheme-r16 ENUMERATED {supported} OPTIONAL

}

FeatureSetDownlink-v1700 ::= SEQUENCE {

 -- R1 36-2: Scaling factor to be applied to 1024QAM for FR1

 scalingFactor-1024QAM-FR1-r17 ENUMERATED {f0p4, f0p75, f0p8} OPTIONAL,

 -- R1 24 feature for existing UE cap to include new SCS

 timeDurationForQCL-v1710 SEQUENCE {

 scs-480kHz ENUMERATED {s56, s112} OPTIONAL,

 scs-960kHz ENUMERATED {s112, s224} OPTIONAL

 } OPTIONAL,

 -- R1 23-6-1 SFN scheme A (scheme 1) for PDSCH and PDCCH

 sfn-SchemeA-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 23-6-1-1 SFN scheme A (scheme 1) for PDCCH only

 sfn-SchemeA-PDCCH-only-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 23-6-1a Dynamic switching - scheme A

 sfn-SchemeA-DynamicSwitching-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 23-6-1b SFN scheme A (scheme 1) for PDSCH only

 sfn-SchemeA-PDSCH-only-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 23-6-2 SFN scheme B (TRP based pre-compensation) for PDSCH and PDCCH

 sfn-SchemeB-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 23-6-2a Dynamic switching - scheme B

 sfn-SchemeB-DynamicSwitching-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 23-6-2b SFN scheme B (TRP based pre-compensation) for PDSCH only

 sfn-SchemeB-PDSCH-only-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 23-2-1d PDCCH repetition for Case 2 PDCCH monitoring with a span gap

 mTRP-PDCCH-Case2-1SpanGap-r17 SEQUENCE {

 scs-15kHz-r17 PDCCH-RepetitionParameters-r17 OPTIONAL,

 scs-30kHz-r17 PDCCH-RepetitionParameters-r17 OPTIONAL,

 scs-60kHz-r17 PDCCH-RepetitionParameters-r17 OPTIONAL,

 scs-120kHz-r17 PDCCH-RepetitionParameters-r17 OPTIONAL

 } OPTIONAL,

 -- R1 23-2-1e PDCCH repetition for Rel-16 PDCCH monitoring

 mTRP-PDCCH-legacyMonitoring-r17 SEQUENCE {

 scs-15kHz-r17 PDCCH-RepetitionParameters-r17 OPTIONAL,

 scs-30kHz-r17 PDCCH-RepetitionParameters-r17 OPTIONAL

 } OPTIONAL,

 -- R1 23-2-4 Simultaneous configuration of PDCCH repetition and multi-DCI based multi-TRP

 mTRP-PDCCH-multiDCI-multiTRP-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 33-2: Dynamic scheduling for multicast for PCell

 dynamicMulticastPCell-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 23-2-1 PDCCH repetition

 mTRP-PDCCH-Repetition-r17 SEQUENCE {

 numBD-twoPDCCH-r17 INTEGER (2..3),

 maxNumOverlaps-r17 ENUMERATED {n1,n2,n3,n5,n10,n20,n40}

 } OPTIONAL

}

FeatureSetDownlink-v1720 ::= SEQUENCE {

 -- R1 25-19: RTT-based Propagation delay compensation based on CSI-RS for tracking and SRS

 rtt-BasedPDC-CSI-RS-ForTracking-r17 ENUMERATED {supported} OPTIONAL,

 -- R1 25-19a: RTT-based Propagation delay compensation based on DL PRS for RTT-based PDC and SRS

 rtt-BasedPDC-PRS-r17 SEQUENCE {

 maxNumberPRS-Resource-r17 ENUMERATED {n1, n2, n4, n8, n16, n32, n64},

 maxNumberPRS-ResourceProcessedPerSlot-r17 SEQUENCE {

 scs-15kHz-r17 ENUMERATED {n1, n2, n4, n6, n8, n12, n16, n24, n32, n48, n64} OPTIONAL,

 scs-30kHz-r17 ENUMERATED {n1, n2, n4, n6, n8, n12, n16, n24, n32, n48, n64} OPTIONAL,

 scs-60kHz-r17 ENUMERATED {n1, n2, n4, n6, n8, n12, n16, n24, n32, n48, n64} OPTIONAL,

 scs-120kHz-r17 ENUMERATED {n1, n2, n4, n6, n8, n12, n16, n24, n32, n48, n64} OPTIONAL

 }

 } OPTIONAL,

 -- R1 33-5-1: SPS group-common PDSCH for multicast on PCell

 sps-Multicast-r17 ENUMERATED {supported} OPTIONAL

}

FeatureSetDownlink-v1730 ::= SEQUENCE {

 -- R1 25-19b: Support of PRS as spatial relation RS for SRS

 prs-AsSpatialRelationRS-For-SRS-r17 ENUMERATED {supported} OPTIONAL

}

FeatureSetDownlink-v1800 ::= SEQUENCE {

 -- R1 40-4-1: Basic feature of Rel.18 enhanced DMRS ports for PDSCH for mapping type A

 pdsch-TypeA-DMRS-r18 ENUMERATED {supported} OPTIONAL,

 -- R1 40-4-1a: Basic feature of Rel.18 enhanced DMRS ports for PDSCH for mapping type B

 pdsch-TypeB-DMRS-r18 ENUMERATED {supported} OPTIONAL,

 -- R1 40-4-1b: 1 symbol FL DMRS and 2 additional DMRS symbols for more than one port for Rel.18 enhanced DMRS ports for PDSCH

 pdsch-1SymbolFL-DMRS-Addition2Symbol-r18 ENUMERATED {supported} OPTIONAL,

 -- R1 40-4-1c: Alternative additional DMRS position for co-existence with LTE CRS for Rel.18 enhanced DMRS ports for PDSCH

 pdsch-AlternativeDMRS-Coexistence-r18 ENUMERATED {supported} OPTIONAL,

 -- R1 40-4-1d: 2 symbols FL-DMRS for Rel.18 enhanced DMRS ports for PDSCH

 pdsch-2SymbolFL-DMRS-r18 ENUMERATED {supported} OPTIONAL,

 -- R1 40-4-1e: 2-symbol FL DMRS + one additional 2-symbols DMRS for Rel.18 enhanced DMRS ports for PDSCH

 pdsch-2SymbolFL-DMRS-Addition2Symbol-r18 ENUMERATED {supported} OPTIONAL,

 -- R1 40-4-1f: 1 symbol FL DMRS and 3 additional DMRS symbols for Rel.18 enhanced DMRS ports for PDSCH

 pdsch-1SymbolFL-DMRS-Addition3Symbol-r18 ENUMERATED {supported} OPTIONAL,

 -- R1 40-4-1g: DMRS type for Rel.18 enhanced DMRS ports for PDSCH

 pdsch-DMRS-Type-r18 ENUMERATED {etype1, etype1And2} OPTIONAL,

 -- R1 40-4-1h: 1 port DL PTRS for Rel.18 enhanced DMRS ports for PDSCH with rank 1-8

 pdsch-1PortDL-PTRS-r18 ENUMERATED {supported} OPTIONAL,

 -- R1 40-4-1i: 2 port DL PTRS for Rel.18 enhanced DMRS ports for PDSCH with rank 1-8

 pdsch-2PortDL-PTRS-r18 ENUMERATED {supported} OPTIONAL,

 -- R1 40-4-1j: Support 1 symbol FL DMRS and 2 additional DMRS symbols for at least one port for mapping type A

 mappingTypeA-1SymbolFL-DMRS-Addition2Symbol-r18 ENUMERATED {supported} OPTIONAL,

 -- R1 40-4-4: Reception of PDSCH without the scheduling restriction for Rel.18 eType1 DMRS ports

 pdsch-ReceptionWithoutSchedulingRestriction-r18 ENUMERATED {supported} OPTIONAL,

 -- R1 40-4-4a: Reception of PDSCH without the scheduling restriction for Rel.18 eType1 DMRS ports for PDSCH with fdmSchemeA

 pdsch-ReceptionSchemeA-r18 ENUMERATED {supported} OPTIONAL,

 -- R1 40-4-4b: Reception of PDSCH without the scheduling restriction for Rel.18 eType1 DMRS ports for PDSCH with fdmSchemeB

 pdsch-ReceptionSchemeB-r18 ENUMERATED {supported} OPTIONAL,

 -- R1 40-4-5: Rel-18 DL DMRS with single DCI based M-TRP

 dmrs-MultiTRP-SingleDCI-r18 ENUMERATED {supported} OPTIONAL,

 -- R1 40-4-5a: Additional row(s) for antenna ports (0,2,3) for Rel.18 DMRS ports for single-DCI based M-TRP

 dmrs-MultiTRP-AddtionRows-r18 ENUMERATED {supported} OPTIONAL,

 -- R1 40-4-7: Rel-18 DL DMRS with M-DCI based M-TRP

 dmrs-MultiTRP-MultiDCI-r18 ENUMERATED {supported} OPTIONAL,

 -- R1 40-4-12: Support of Rel-18 DMRS and PDSCH processing capability 2 simultaneously

 simulDMRS-PDSCH-r18 SEQUENCE {

 scs-15kHz-r18 INTEGER (0..4) OPTIONAL,

 scs-30kHz-r18 INTEGER (0..5) OPTIONAL,

 scs-60kHz-r18 INTEGER (0..7) OPTIONAL

 } OPTIONAL,

 -- R1 53-1: Support RLM/BM/BFD and gapless L3 intra-frequency measurements based on CD-SSB outside active BWP without interruptions

 bwpOperationMeasWithoutInterrupt-r18 ENUMERATED {supported} OPTIONAL,

 -- R1 55-6: (2, 2) span-based PDCCH monitoring with additional restriction(s)

 pdcch-MonitoringSpan2-2-r18 SEQUENCE{

 pdsch-ProcessingType1-r18 SEQUENCE{

 scs-15kHz-r18 ENUMERATED {supported} OPTIONAL,

 scs-30kHz-r18 ENUMERATED {supported} OPTIONAL

 },

 pdsch-ProcessingType2-r18 SEQUENCE{

 scs-15kHz-r18 ENUMERATED {supported} OPTIONAL,

 scs-30kHz-r18 ENUMERATED {supported} OPTIONAL

 }

 } OPTIONAL,

 -- R1 55-6b: Mix of Rel-16 PDCCH monitoring capability and Rel. 15 PDCCH monitoring capability on different carriers

 pdcch-MonitoringMixed-r18 ENUMERATED {supported} OPTIONAL,

 -- R4 42-1: Support of SCell without SS/PBCH block for inter-band CA

 scellWithoutSSB-InterBandCA-r18 CHOICE {

 supportOfSingleGroup ENUMERATED {referenceBand, scellWithoutSSB, both},

 supportOfMultipleGroups ENUMERATED {referenceBand1, scellWithoutSSB1, referenceBand2, scellWithoutSSB2}

 } OPTIONAL,

 multicastInactive-r18 ENUMERATED {supported} OPTIONAL,

 thresholdBasedMulticastResume-r18 ENUMERATED {supported} OPTIONAL

}

PDCCH-MonitoringOccasions-r16 ::= SEQUENCE {

 period7span3-r16 ENUMERATED {supported} OPTIONAL,

 period4span3-r16 ENUMERATED {supported} OPTIONAL,

 period2span2-r16 ENUMERATED {supported} OPTIONAL

}

PDCCH-RepetitionParameters-r17 ::= SEQUENCE {

 supportedMode-r17 ENUMERATED {intra-span, inter-span, both},

 limitX-PerCC-r17 ENUMERATED {n4, n8, n16, n32, n44, n64, nolimit} OPTIONAL,

 limitX-AcrossCC-r17 ENUMERATED {n4, n8, n16, n32, n44, n64, n128, n256, n512, nolimit} OPTIONAL

}

DummyA ::= SEQUENCE {

 maxNumberNZP-CSI-RS-PerCC INTEGER (1..32),

 maxNumberPortsAcrossNZP-CSI-RS-PerCC ENUMERATED {p2, p4, p8, p12, p16, p24, p32, p40, p48, p56, p64, p72, p80,

 p88, p96, p104, p112, p120, p128, p136, p144, p152, p160, p168,

 p176, p184, p192, p200, p208, p216, p224, p232, p240, p248, p256},

 maxNumberCS-IM-PerCC ENUMERATED {n1, n2, n4, n8, n16, n32},

 maxNumberSimultaneousCSI-RS-ActBWP-AllCC ENUMERATED {n5, n6, n7, n8, n9, n10, n12, n14, n16, n18, n20, n22, n24, n26,

 n28, n30, n32, n34, n36, n38, n40, n42, n44, n46, n48, n50, n52,

 n54, n56, n58, n60, n62, n64},

 totalNumberPortsSimultaneousCSI-RS-ActBWP-AllCC ENUMERATED {p8, p12, p16, p24, p32, p40, p48, p56, p64, p72, p80,

 p88, p96, p104, p112, p120, p128, p136, p144, p152, p160, p168,

 p176, p184, p192, p200, p208, p216, p224, p232, p240, p248, p256}

}

DummyB ::= SEQUENCE {

 maxNumberTxPortsPerResource ENUMERATED {p2, p4, p8, p12, p16, p24, p32},

 maxNumberResources INTEGER (1..64),

 totalNumberTxPorts INTEGER (2..256),

 supportedCodebookMode ENUMERATED {mode1, mode1AndMode2},

 maxNumberCSI-RS-PerResourceSet INTEGER (1..8)

}

DummyC ::= SEQUENCE {

 maxNumberTxPortsPerResource ENUMERATED {p8, p16, p32},

 maxNumberResources INTEGER (1..64),

 totalNumberTxPorts INTEGER (2..256),

 supportedCodebookMode ENUMERATED {mode1, mode2, both},

 supportedNumberPanels ENUMERATED {n2, n4},

 maxNumberCSI-RS-PerResourceSet INTEGER (1..8)

}

DummyD ::= SEQUENCE {

 maxNumberTxPortsPerResource ENUMERATED {p4, p8, p12, p16, p24, p32},

 maxNumberResources INTEGER (1..64),

 totalNumberTxPorts INTEGER (2..256),

 parameterLx INTEGER (2..4),

 amplitudeScalingType ENUMERATED {wideband, widebandAndSubband},

 amplitudeSubsetRestriction ENUMERATED {supported} OPTIONAL,

 maxNumberCSI-RS-PerResourceSet INTEGER (1..8)

}

DummyE ::= SEQUENCE {

 maxNumberTxPortsPerResource ENUMERATED {p4, p8, p12, p16, p24, p32},

 maxNumberResources INTEGER (1..64),

 totalNumberTxPorts INTEGER (2..256),

 parameterLx INTEGER (2..4),

 amplitudeScalingType ENUMERATED {wideband, widebandAndSubband},

 maxNumberCSI-RS-PerResourceSet INTEGER (1..8)

}

-- TAG-FEATURESETDOWNLINK-STOP

-- ASN1STOP

|  |
| --- |
| ***FeatureSetDownlink* field descriptions** |
| ***featureSetListPerDownlinkCC***Indicates which features the UE supports on the individual DL carriers of the feature set (and hence of a band entry that refer to the feature set). The UE shall hence include at least as many *FeatureSetDownlinkPerCC-Id* in this list as the number of carriers it supports according to the *ca-BandwidthClassDL*, except if indicating additional functionality by reducing the number of *FeatureSetDownlinkPerCC-Id* in the feature set (see NOTE 1 in *FeatureSetCombination* IE description). The order of the elements in this list is not relevant, i.e., the network may configure any of the carriers in accordance with any of the *FeatureSetDownlinkPerCC-Id* in this list. |
| ***supportedSRS-Resources***Indicates supported SRS resources for SRS carrier switching to the band associated with this *FeatureSetDownlink*. The UE is only allowed to set this field for a band with associated *FeatureSetUplinkId* set to 0. |

**END OF THE CHANGE**