Companies providing input to this email discussion are requested to leave contact information below.

|  |  |  |
| --- | --- | --- |
| **Company** | **Delegate name** | **Email address** |
| ASUSTeK | Lider Pan | lider\_pan@asus.com |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

# 1 Comments on CR

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Company** | **Clause number** | **Original text in CR** | **Suggested modification or comments** | **Rapporteur response** |
| ASUSTeK | 5.8.9.2.3 | NOTE 3: It is up to UE implementation whether to include fields other than *pdcp-ParametersSidelink* in the *UECapabilityInformationSidelink* message for for end-to-end L2 U2U relay NR sidelink communication. | Since setting the contents of *UECapabilityInformationSidelink* message is specified in clause 5.8.9.2.4, the new note (i.e. NOTE 3) added in clause 5.8.9.2.3 should be moved to clause 5.8.9.2.4.  In addition, there is a redundant word (i.e. “for”) in this new note. |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

# 2 Comments on RIL list

|  |  |  |
| --- | --- | --- |
| **Company** | **Suggested modification or comments** | **Rapporteur response** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |