|  |  |  |
| --- | --- | --- |
| **Company** | **Comment** | **Rapp Response**  |
| OPPO | 5.22.1.13> else if one or more HARQ retransmissions are selected and the selected resource pool is not Dedicated SL-PRS resource pool and no resources were selected for more than one transmission opportunities:This addition would lead to consequence that **if MCSt is used, there is no chance for UE to enter into the HARQ re-transmission branch**, which is wrong, since based on the NOTE below, there is for sure a case where even if MCSt is used, HARQ re-transmission is also usedNOTE 3Aa: For Multi-consecutive slots transmission as specified in clause 8.1.4 of TS 38.214 [7], during resource (re)selection, leave it to UE implementation, regarding whether to calculate the number of HARQ retransmissions from the allowed numbers based on the number of MCSt transmissions, or the number of slot(s) within Multi-consecutive slots transmission. |  |
| OPPO | 5.22.1.1NOTE 3B8: UE is not expected to be (pre-)configured with both random selection and sl-NRPSSCH-EUTRA-ThresRSRP-List in the same resource pool applies only to NR SL normal resource pool. This does not apply to the NR SL exceptional pool.It seems more a restriction to be captured by RRC? But no strong view, if we go with MAC, some minor rewording. |  |
| OPPO |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |