**3GPP TSG- WG2 Meeting #130 *R2-250xxxx***

**St Julian’s, Malta,**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.3* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  |  | **CR** | **draft** | **rev** | **-** | **Current version:** |  |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **x** | Radio Access Network |  | Core Network | **x** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Running CR for AI/ML Positioning Accuracy Enhancements | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Qualcomm Incorporated (Rapporteur) | | | | | | | | | |
| ***Source to TSG:*** |  | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | -Core | | | | |  | ***Date:*** | | | 2025-05-08 |
|  |  | | | |  | |  | | |  |
| ***Category:*** |  |  | | | | | ***Release:*** | | |  |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)  Rel-20 (Release 20)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | Introduce support for AI/ML positioning accuracy enhancements. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | TBD | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | AI/ML positioning accuracy enhancements cannot be supported. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | TBD | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | | **x** |  | Other core specifications | | | | TS/TR TBD CR ... | | |
| ***affected:*** | |  | **x** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | | RAN2#129bis: First version v00 in R2-2502618.  RAN2#130: v01 updates based on [POST129bis][015][AI PHY] discussion.   TBD | | | | | | | | |

# Foreword

This Technical Specification has been produced by the 3rd Generation Partnership Project (3GPP).

The contents of the present document are subject to continuing work within the TSG and may change following formal TSG approval. Should the TSG modify the contents of the present document, it will be re-released by the TSG with an identifying change of release date and an increase in version number as follows:

Version x.y.z

where:

x the first digit:

1 presented to TSG for information;

2 presented to TSG for approval;

3 or greater indicates TSG approved document under change control.

y the second digit is incremented for all changes of substance, i.e. technical enhancements, corrections, updates, etc.

z the third digit is incremented when editorial only changes have been incorporated in the document.

# 1 Scope

The present document contains the definition of the LTE Positioning Protocol (LPP) for the radio access technologies E-UTRA/LTE and NR.

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications".

[2] 3GPP TS 36.305: "Stage 2 functional specification of User Equipment (UE) positioning in E-UTRAN".

[3] 3GPP TS 23.271: "Functional stage 2 description of Location Services (LCS)".

[4] IS-GPS-200, Revision D, Navstar GPS Space Segment/Navigation User Interfaces, March 7th, 2006.

[5] IS-GPS-705, Navstar GPS Space Segment/User Segment L5 Interfaces, September 22, 2005.

[6] IS-GPS-800, Navstar GPS Space Segment/User Segment L1C Interfaces, September 4, 2008.

[7] IS-QZSS, Quasi Zenith Satellite System Navigation Service Interface Specifications for QZSS, Ver.1.1, July 31, 2009.

[8] Galileo OS Signal in Space ICD (OS SIS ICD), Issue 1.2, February 2014, European Union.

[9] Global Navigation Satellite System GLONASS Interface Control Document, Version 5.1, 2008.

[10] Specification for the Wide Area Augmentation System (WAAS), US Department of Transportation, Federal Aviation Administration, DTFA01-96-C-00025, 2001.

[11] RTCM-SC104, RTCM Recommended Standards for Differential GNSS Service (v.2.3), August 20, 2001.

[12] 3GPP TS 36.331: "Evolved Universal Terrestrial Radio Access (E-UTRA); "Radio Resource Control (RRC); Protocol specification".

[13] 3GPP TS 25.331: "Radio Resource Control (RRC); Protocol Specification".

[14] 3GPP TS 44.031: "Location Services (LCS); Mobile Station (MS) - Serving Mobile Location Centre (SMLC) Radio Resource LCS Protocol (RRLP)".

[15] 3GPP TS 23.032: "Universal Geographical Area Description (GAD)".

[16] 3GPP TS 36.211: "Evolved Universal Terrestrial Radio Access (E-UTRA); Physical Channels and Modulation".

[17] 3GPP TS 36.214: "Evolved Universal Terrestrial Radio Access (E-UTRA); Physical layer – Measurements".

[18] 3GPP TS 36.133: "Evolved Universal Terrestrial Radio Access (E-UTRA); Requirements for support of radio resource management".

[19] 3GPP TS 23.003: "Numbering, addressing and identification".

[20] OMA-TS-LPPe-V1\_0, LPP Extensions Specification, Open Mobile Alliance.

[21] 3GPP TS 36.101: "Evolved Universal Terrestrial Radio Access (E-UTRA); User Equipment (UE) radio transmission and reception".

[22] ITU-T Recommendation X.691 (07/2002) "Information technology - ASN.1 encoding rules: Specification of Packed Encoding Rules (PER)" (Same as the ISO/IEC International Standard 8825-2).

[23] BDS-SIS-ICD-B1I-3.0: "BeiDou Navigation Satellite System Signal In Space Interface Control Document Open Service Signal B1I (Version 3.0)", February, 2019.

[24] ATIS-0500027: "Recommendations for Establishing Wide Scale Indoor Location Performance", May 2015.

[25] Bluetooth Special Interest Group: "Bluetooth Core Specification v4.2", December 2014.

[26] IEEE 802.11, Part 11: "Wireless LAN Medium Access Control (MAC) and Physical Layer (PHY) Specifications".

[27] IETF RFC 6225, "Dynamic Host Configuration Protocol Options for Coordinate-Based Location Configuration Information", July 2011.

[28] 3GPP TS 36.213: "Evolved Universal Terrestrial Radio Access (E-UTRA); Physical layer procedures".

[29] "Earth Gravitational Model 96 (EGM96)", National Geospatial-Intelligence Agency, NASA.

[30] RTCM Standard 10403.3: "Differential GNSS (Global Navigation Satellite Systems) Services" – Version 3, October 7, 2016.

[31] IGS ANTEX: "The Antenna Exchanged Format" – version 1.4, September 15, 2010.

[32] Federal Information Processing Standards Publication 197, "Specification for the ADVANCED ENCRYPTION STANDARD (AES)", November 26, 2001.

[33] NIST Special Publication 800-38A, "Recommendation for Block Cipher Modes of Operation Methods and Techniques", 2001.

[34] 3GPP TS 38.101-2: "NR; User Equipment (UE) radio transmission and reception; Part 2: Range 2 Standalone".

[35] 3GPP TS 38.331: "NR; Radio Resource Control (RRC); Protocol specification".

[36] 3GPP TS 38.215: "NR; Physical layer measurements".

[37] 3GPP TS 38.101-1: "NR; User Equipment (UE) radio transmission and reception; Part 1: Range 1 Standalone".

[38] IRNSS Signal-In-Space (SPS) Interface Control Document (ICD) for standard positioning service version 1.1, Aug 2017.

[39] BDS-SIS-ICD-B1C-1.0: "BeiDou Navigation Satellite System Signal In Space Interface Control Document Open Service Signal B1C (Version 1.0)", December, 2017.

[40] 3GPP TS 38.305: "NG Radio Access Network (NG-RAN); Stage 2 functional specification of User Equipment (UE) positioning in NG-RAN".

[41] 3GPP TS 38.211: "3rd Generation Partnership Project; Technical Specification Group Radio Access Network; NR; Physical channels and modulation".

[42] 3GPP TS 23.273: "5G System (5GS) Location Services (LCS); Stage 2".

[43] IS-QZSS-L6-001, Quasi-Zenith Satellite System Interface Specification – Centimetre Level Augmentation Service, Cabinet Office, November 5, 2018.

[44] 3GPP TR 38.901: "Technical Specification Group Radio Access Network; Study on channel model for frequencies from 0.5 to 100 GHz".

[45] 3GPP TS 38.214: "NR; Physical layer procedures for data".

[46] 3GPP TS 38.133: "NR; Requirements for support of radio resource management".

[47] 3GPP TS 38.300: "NR; NR and NG-RAN Overall Description; Stage 2".

[48] 3GPP TS 38.213: "NR; Physical layer procedures for control".

[49] BDS-SIS-ICD-B2a-1.0: "BeiDou Navigation Satellite System Signal In Space Interface Control Document Open Service Signal B2a (Version 1.0)", December, 2017.

[50] BDS-SIS-ICD-B3I-1.0: "BeiDou Navigation Satellite System Signal In Space Interface Control Document Open Service Signal B3I (Version 1.0)", February, 2018.

[51] NMEA standard 0183, Version 4.11, November 2018.

[52] BDS-SIS-ICD-PPP-B2b-1.0: "BeiDou Navigation Satellite System Signal In Space Interface Control Document Precise Point Positioning Service Signal PPP-B2b (Version 1.0)", July, 2020.

[53] Bluetooth Special Interest Group: "Bluetooth Core Specification v5.4", February 2023.

[54] 3GPP TS 38.101-5: "User Equipment (UE) radio transmission and reception; Part 5: Satellite access Radio Frequency (RF) and performance requirements".

# 3 Definitions and Abbreviations

## 3.1 Definitions

For the purposes of the present document, the terms and definitions given in TR 21.905 [1], TS 36.305 [2], TS 23.271 [3], 38.305 [40] and TS 23.273 [42] apply. Other definitions are provided below.

**Anchor carrier:** In NB-IoT, a carrier where the UE assumes that NPSS/NSSS/NPBCH/SIB-NB for FDD or NPSS/NSSS/NPBCH for TDD are transmitted.

**Location Server:** a physical or logical entity (e.g., E-SMLC, SUPL SLP, or LMF) that manages positioning for a target device by obtaining measurements and other location information from one or more positioning units and providing assistance data to positioning units to help determine this. A Location Server may also compute or verify the final location estimate.

**NB-IoT:** NB-IoT allows access to network services via E-UTRA with a channel bandwidth limited to 200 kHz.

**Observed Time Difference Of Arrival (OTDOA):** The time interval that is observed by a target device between the reception of downlink signals from two different TPs. If a signal from TP 1 is received at the moment *t1*, and a signal from TP 2 is received at the moment *t2*, the OTDOA is *t2* – *t1*.

**Positioning frequency layer**: A positioning frequency layer is defined as a collection of DL-PRS Resource Sets where each DL-PRS Resource Set is in turn a collection of DL-PRS Resources. All DL-PRS Resources from all DL-PRS Resource Sets from the same positioning frequency layer have some common/same DL-PRS parameters viz. DL-PRS subcarrier spacing, DL-PRS Resource bandwidth, DL-PRS start PRB, DL-PRS Point A, DL-PRS Comb size and DL-PRS cyclic prefix.

**PRS-only TP**: A TP which only transmits PRS signals or DL-PRS for PRS-based TBS positioning and is not associated with a cell.

**Reference Source:** a physical entity or part of a physical entity that provides signals (e.g., RF, acoustic, infra-red) that can be measured (e.g., by a Target Device) in order to obtain the location of a Target Device.

**Relative Time Difference (RTD):** The relative time difference between a TRP *i* and a TRP *j*, is defined as *tj – ti*, where *ti* and *tj* are defined as the time when TRP *i* and *j* transmit the start of one subframe respectively.

**Rx Time Delay:** From a signal reception perspective, there will be a time delay from the time when the RF signal arrives at the Rx antenna to the time when the signal is digitized and time-stamped at the baseband.

**Rx Timing Error:** Result of Rx Time Delay involved in the reception of a signal before reporting measurements that are obtained from the signal. It is the uncalibrated Rx Time Delay, or the remaining delay after the UE/TRP internal calibration/compensation of the Rx Time Delay, involved in the reception of the DL-PRS/UL SRS signals. The calibration/compensation may also include the calibration/compensation of the relative time delay between different RF chains in the same UE/TRP and may also possibly consider the offset of the Rx antenna phase centre to the physical antenna centre.

**Target Device:** the device that is being positioned (e.g., UE or SUPL SET).

**Transmission Point (TP):** A set of geographically co-located transmit antennas (e.g. antenna array (with one or more antenna elements)) for one cell, part of one cell or one PRS-only TP. Transmission Points can include base station (eNodeB) antennas, remote radio heads, a remote antenna of a base station, an antenna of a PRS-only TP, etc. One cell can be formed by one or multiple transmission points. For a homogeneous deployment, each transmission point may correspond to one cell.

**Transmission-Reception Point (TRP)**: A set of geographically co-located antennas (e.g. antenna array (with one or more antenna elements)) supporting TP and/or RP functionality.

**TRP Tx Timing Error Group (TRP Tx TEG):** Tx Timing Errors, associated with TRP transmissions on one or more DL-PRS Resources, that are within a certain margin.

**Tx Time Delay:** From a signal transmission perspective, the time delay from the time when the digital signal is generated at baseband to the time when the RF signal is transmitted from the Tx antenna.

**Tx Timing Error:** Result of Tx Time Delay involved in the transmission of a signal. It is the uncalibrated Tx Time Delay, or the remaining delay after the TRP/UE internal calibration/compensation of the Tx Time Delay, involved in the transmission of the DL-PRS/UL SRS signals. The calibration/compensation may also include the calibration/compensation of the relative time delay between different RF chains in the same TRP/UE and may also possibly consider the offset of the Tx antenna phase centre to the physical antenna centre.

**UE Rx Timing Error Group (UE Rx TEG)**: Rx Timing Errors, associated with UE reporting of one or more DL measurements, that are within a certain margin.

**UE RxTx Timing Error Group (UE RxTx TEG):** Rx Timing Errors and Tx Timing Errors, associated with UE reporting of one or more UE Rx-Tx time difference measurements, which have the 'Rx Timing Errors + Tx Timing Errors' differences within a certain margin.

**UE Tx Timing Error Group (UE Tx TEG)**: Tx Timing Errors, associated with UE transmissions on one or more UL SRS resources for positioning purpose, that are within a certain margin.

## 3.2 Abbreviations

For the purposes of the present document, the following abbreviations apply.

ADR Accumulated Delta-Range

A‑GNSS Assisted‑GNSS

AI Artificial Intelligence

AoA Angle-of-Arrival

AoD Angle-of-Departure

AP Access Point

ARFCN Absolute Radio Frequency Channel Number

ARP Antenna Reference Point

BDS BeiDou Navigation Satellite System

BIPM Bureau International des Poids et Mesures (International Bureau of Weights and Measures)

BSSID Basic Service Set Identifier

BTS Base Transceiver Station (GERAN)

CID Cell-ID (positioning method)

CNAV Civil Navigation

CRS Cell-specific Reference Signals

DL-AoD Downlink Angle-of-Departure

DL-TDOA Downlink Time Difference Of Arrival

ECEF Earth-Centered, Earth-Fixed

ECGI Evolved Cell Global Identifier

ECI Earth-Centered-Inertial

E‑CID Enhanced Cell-ID (positioning method)

EGNOS European Geostationary Navigation Overlay Service

E-SMLC Enhanced Serving Mobile Location Centre

E-UTRA Evolved Universal Terrestrial Radio Access

E-UTRAN Evolved Universal Terrestrial Radio Access Network

EOP Earth Orientation Parameters

EPDU External Protocol Data Unit

FDMA Frequency Division Multiple Access

FEC Forward Error Correction

FKP (German) Flächen-Korrektur-Parameter (area correction parameter)

FTA Fine Time Assistance

GAGAN GPS Aided Geo Augmented Navigation

GLONASS GLObal'naya NAvigatsionnaya Sputnikovaya Sistema (Engl.: Global Navigation Satellite System)

GNSS Global Navigation Satellite System

GPS Global Positioning System

HA GNSS High-Accuracy GNSS (RTK, PPP)

HPL Horizontal Protection Level

ICD Interface Control Document

IGS International GNSS Service

IOD Issue of Data

IRNSS Indian Regional Navigation Satellite System

IS Interface Specification

LLA Latitude Longitude Altitude

LMF Location Management Function

LOS Line-of-Sight

LPP LTE Positioning Protocol

LPPa LTE Positioning Protocol Annex

LSB Least Significant Bit

MAC Master Auxiliary Concept

MBS Metropolitan Beacon System

MG Measurement Gap

ML Machine Learning

MO-LR Mobile Originated Location Request

MSAS Multi-functional Satellite Augmentation System

MSB Most Significant Bit

msd mean solar day

MT-LR Mobile Terminated Location Request

Multi-RTT Multiple-Round Trip Time

NAV Navigation

NavIC NAVigation with Indian Constellation

NB-IoT NarrowBand Internet of Things

NCGI NR Cell Global Identifier

NICT National Institute of Information and Communications Technology

NI-LR Network Induced Location Request

NLOS Non-Line-of-Sight

NPRS Narrowband Positioning Reference Signals

NR NR Radio Access

NRSRP Narrowband Reference Signal Received Power

NRSRQ Narrowband Reference Signal Received Quality

NTN Non-Terrestrial Network

NTSC National Time Service Center of Chinese Academy of Sciences

OSR Observation Space Representation

OTDOA Observed Time Difference Of Arrival

PBCH Physical Broadcast Channel

PDU Protocol Data Unit

PFL Positioning Frequency Layer

PL Protection Level

PPP Precise Point Positioning

PPW PRS Processing Window

PRB Physical Resource Block

PRC Pseudo‑Range Correction

PRS Positioning Reference Signals

posSIB Positioning System Information Block

PRU Positioning Reference Unit

PZ-90 Parametry Zemli 1990 Goda – Parameters of the Earth Year 1990

QCL Quasi Co-Location

QZS Quasi Zenith Satellite

QZSS Quasi-Zenith Satellite System

QZST Quasi-Zenith System Time

RF Radio Frequency

RP Reception Point

RRC Range‑Rate Correction

Radio Resource Control

RSCP Reference Signal Carrier Phase

RSCPD Reference Signal Carrier Phase Difference

RSRP Reference Signal Received Power

RSRPP Reference Signal Received Path Power

RSRQ Reference Signal Received Quality

RSTD Reference Signal Time Difference

RTK Real-Time Kinematic

RTT Round Trip Time

RU Russia

SBAS Space Based Augmentation System

SET SUPL Enabled Terminal

SFN System Frame Number

SLP SUPL Location Platform

SRS Sounding Reference Signal

SS Synchronization Signal

SSB Synchronization Signal Block, SS/PBCH Block

SSID Service Set Identifier

SSR State Space Representation

STEC Slant TEC

SUPL Secure User Plane Location

SV Space Vehicle

TB Terrestrial Beacon

TBS Terrestrial Beacon System

TEC Total Electron Content

TECU TEC Units

TEG Timing Error Group

TIR Target Integrity Risk

TLM Telemetry

TOA Time Of Arrival

TOD Time Of Day

TOW Time Of Week

TP Transmission Point

TRP Transmission-Reception Point

UDRE User Differential Range Error

ULP User Plane Location Protocol

URA User Range Accuracy

USNO US Naval Observatory

UT1 Universal Time No.1

UTC Coordinated Universal Time

VPL Vertical Protection Level

WAAS Wide Area Augmentation System

WGS‑84 World Geodetic System 1984

WLAN Wireless Local Area Network

# 4 Functionality of Protocol

## 4.1 General

### 4.1.1 LPP Configuration

LPP is used point-to-point between a location server (E-SMLC, LMF or SLP) and a target device (UE or SET) in order to position the target device using position-related measurements obtained by one or more reference sources. Figure 4.1.1-1 shows the configuration as applied to the control- and user-plane location solutions for E-UTRAN and NG-RAN (as defined in TS 36.305 [2], TS 38.305 [40], TS 23.273 [42] and TS 23.271 [3]).

LPP is also used point-to-point between a location server and a PRU. In this specification, procedures and messages specified for the target device equally apply to a PRU, as specified in TS 23.273 [42].

NB-IoT is a non-backward compatible variant of E-UTRAN supporting a reduced set of functionalities. In this specification, procedures and messages specified for the UE equally apply to the UE in NB-IoT.



Figure 4.1.1-1: LPP Configuration for Control- and User-Plane Positioning in E-UTRAN or NG-RAN

### 4.1.2 LPP Sessions and Transactions

An LPP session is used between a Location Server and the target device in order to obtain location related measurements or a location estimate or to transfer assistance data. A single LPP session is used to support a single location request (e.g., for a single MT-LR, MO-LR or NI-LR). Multiple LPP sessions can be used between the same endpoints to support multiple different location requests (as required by TS 23.271 [3]). Each LPP session comprises one or more LPP transactions, with each LPP transaction performing a single operation (capability exchange, assistance data transfer, or location information transfer). In E-UTRAN and NG-RAN, the LPP transactions are realized as LPP procedures. The instigator of an LPP session will always instigate the first LPP transaction, but subsequent transactions may be instigated by either end. LPP transactions within a session may occur serially or in parallel. LPP transactions are indicated at the LPP protocol level with a transaction ID in order to associate messages with one another (e.g., request and response).

Messages within a transaction are linked by a common transaction identifier.

### 4.1.3 LPP Position Methods

Internal LPP positioning methods and associated signalling content are defined in this specification.

This version of the specification defines OTDOA (based on LTE signals), A-GNSS, E-CID (based on LTE signals), Sensor, TBS, WLAN, Bluetooth, NR E-CID, NR DL-TDOA, NR DL-AoD, NR Multi-RTT, and NR AI/ML positioning methods.

### 4.1.4 LPP Messages

Each LPP transaction involves the exchange of one or more LPP messages between the location server and the target device. The general format of an LPP message consists of a set of common fields followed by a body. The body (which may be empty) contains information specific to a particular message type. Each message type contains information specific to one or more positioning methods and/or information common to all positioning methods.

The common fields are as follows:

|  |  |
| --- | --- |
| Field | **Role** |
| Transaction ID | Identify messages belonging to the same transaction |
| Transaction End Flag | Indicate when a transaction (e.g. one with periodic responses) has ended |
| Sequence Number | Enable detection of a duplicate LPP message at a receiver |
| Acknowledgement | Enable an acknowledgement to be requested and/or returned for any LPP message |

NOTE: Use of the Transaction ID and Transaction End fields conform to the procedures in clause 5 and are independent of the means used to transport LPP messages (e.g., whether using a NAS MO-LR Request, NAS Generic Transport or user-plane solution).

The following message types are defined:

- Request Capabilities;

- Provide Capabilities;

- Request Assistance Data;

- Provide Assistance Data;

- Request Location Information;

- Provide Location Information;

- Abort;

- Error.

## 4.2 Common LPP Session Procedure

The purpose of this procedure is to support an LPP session comprising a sequence of LPP transactions. The procedure is described in Figure 4.2-1.



Figure 4.2-1 LPP Session Procedure

1. Endpoint A, which may be either the target or the server, initiates an LPP session by sending an LPP message for an initial LPP transaction *j* to the other endpoint B (which has an opposite role to A).

2. Endpoints A and B may exchange further messages to continue the transaction started in step 1.

3. Either endpoint may instigate further transactions by sending additional LPP messages.

4. A session is terminated by a final transaction *N* in which LPP messages will be exchanged between the two endpoints.

Within each transaction, all constituent messages shall contain the same transaction identifier. The last message sent in each transaction shall have the IE *endTransaction* set to TRUE. Transactions that occur in parallel shall use different transaction IDs; transaction IDs for completed transactions may be reused at any time after the final message of the previous transaction with the same ID is known to have been received.

## 4.3 LPP Transport

### 4.3.1 Transport Layer Requirements

LPP requires reliable, in-sequence delivery of LPP messages from the underlying transport layers. This clause describes the transport capabilities that are available within LPP. A UE implementing LPP for the control-plane solution shall support LPP reliable transport (including all three of duplicate detection, acknowledgement, and retransmission).

LPP reliable transport functionality is not used in the user-plane solution.

The following requirements in clauses 4.3.2, 4.3.3, and 4.3.4 for LPP reliable transport apply only when the capability is supported.

### 4.3.2 LPP Duplicate Detection

A sender shall include a sequence number in all LPP messages sent for a particular location session. The sequence number shall be distinct for different LPP messages sent in the same direction in the same location session (e.g., may start at zero in the first LPP message and increase monotonically in each succeeding LPP message). Sequence numbers used in the uplink and downlink are independent (e.g., can be the same).

A receiver shall record the most recent received sequence number for each location session. If a message is received carrying the same sequence number as that last received for the associated location session, it shall be discarded. Otherwise (i.e., if the sequence number is different or if no sequence number was previously received or if no sequence number is included), the message shall be processed.

Sending and receiving sequence numbers shall be deleted in a server when the associated location session is terminated and shall be deleted in a target device when there has been no activity for a particular location session for 10 minutes.

NOTE: For LPP control-plane use, a target device can be aware of a location session from information provided at the NAS level for downlink transport of an LPP message.

### 4.3.3 LPP Acknowledgement

#### 4.3.3.1 General

Each LPP message may carry an acknowledgement request and/or an acknowledgement indicator. A LPP message including an acknowledgement request (i.e., that include the IE *ackRequested* set to TRUE) shall also include a sequence number. Upon reception of an LPP message which includes the IE *ackRequested* set to TRUE, a receiver returns an LPP message with an acknowledgement response (i.e., that includes the *ackIndicator* IE set to the same sequence number of the message being acknowledged). An acknowledgement response may contain no LPP message body (in which case only the sequence number being acknowledged is significant); alternatively, the acknowledgement may be sent in an LPP message along with an LPP message body. An acknowledgement is returned for each received LPP message that requested an acknowledgement including any duplicate(s). Once a sender receives an acknowledgement for an LPP message, and provided any included sequence number is matching, it is permitted to send the next LPP message. No message reordering is needed at the receiver since this stop-and-wait method of sending ensures that messages normally arrive in the correct order.

When an LPP message is transported via a NAS MO-LR request, the message does not request an acknowledgement.

#### 4.3.3.2 Procedure related to Acknowledgement

Figure 4.3.3.2-1 shows the procedure related to acknowledgement.



Figure 4.3.3.2-1: LPP Acknowledgement procedure

1. Endpoint A sends an LPP message *N* to Endpoint B which includes the IE *ackRequested* set to TRUE and a sequence number.

2. If LPP message *N* is received and Endpoint B is able to decode the *ackRequested* value and sequence number, Endpoint B shall return an acknowledgement for message *N*. The acknowledgement shall contain the IE *ackIndicator* set to the same sequence number as that in message *N*.

3. When the acknowledgement for LPP message *N* is received and provided the included *ackIndicator* IE matches the sequence number sent in message *N*, Endpoint A sends the next LPP message *N+1* to Endpoint B when this message is available.

### 4.3.4 LPP Retransmission

#### 4.3.4.1 General

This capability builds on the acknowledgement and duplicate detection capabilities. When an LPP message which requires acknowledgement is sent and not acknowledged, it is resent by the sender following a timeout period up to three times. If still unacknowledged after that, the sender aborts all LPP activity for the associated session. The timeout period is determined by the sender implementation but shall not be less than a minimum value of 250 ms.

In addition, for NB-IoT the timeout period may be determined by the sender implementation based on e.g., the coverage level of the UE.

#### 4.3.4.2 Procedure related to Retransmission

Figure 4.3.4.2-1 shows the procedure related to retransmission when combined with acknowledgement and duplicate detection.



Figure 4.3.4.2-1: LPP Retransmission procedure

1. Endpoint A sends an LPP message *N* to Endpoint B for a particular location session and includes a request for acknowledgement along with a sequence number.

2. If LPP message *N* is received and Endpoint B is able to decode the *ackRequested* value and sequence number (regardless of whether the message body can be correctly decoded), Endpoint B shall return an acknowledgement for message *N*. If the acknowledgement is received by Endpoint A (such that the acknowledged message can be identified and sequence numbers are matching), Endpoint A skips steps 3 and 4.

3. If the acknowledgement in step 2 is not received after a timeout period, Endpoint A shall retransmit LPP message *N* and shall include the same sequence number as in step 1.

4. If LPP message *N* in step 3 is received and Endpoint B is able to decode the *ackRequested* value and sequence number (regardless of whether the message body can be correctly decoded and whether or not the message is considered a duplicate), Endpoint B shall return an acknowledgement. Steps 3 may be repeated one or more times if the acknowledgement in step 4 is not received after a timeout period by Endpoint A. If the acknowledgement in step 4 is still not received after sending three retransmissions, Endpoint A shall abort all procedures and activity associated with LPP support for the particular location session.

5. Once an acknowledgement in step 2 or step 4 is received, Endpoint A sends the next LPP message *N+1* for the location session to Endpoint B when this message is available.

### 4.3.5 LPP Message Segmentation

An LPP message body may be sent in several shorter LPP messages instead of one long LPP message to deliver a large amount of information (e.g., in case the LPP message size exceeds the maximum message size supported by lower layers). When a sender employs LPP message segmentation, the sender shall include the IE *SegmentationInfo* in each LPP message segment. The sender shall indicate in all but the final message segment that more messages are on the way.

When a receiver receives an LPP message indicating that more messages are on the way, the receiver may store the LPP message. If the receiver receives a subsequent LPP message for the same session and transaction ID, the receiver shall assume that the new LPP message continues the segmentation of the earlier message and may store the new message if the new message indicates that more messages are on the way. If the new message indicates that no more messages are on the way, the receiver shall assume that message segmentation is complete and shall process the new message and any stored message segments for the same session and transaction ID.

The reliable transport rules specified in clause 4.3.2, 4.3.3, and 4.3.4 apply to each individual LPP message segment, independently of the value of the IE *SegmentationInfo*.

The rules for setting the common fields of the LPP message specified in clause 4.1.4 (Transaction ID, Transaction End Flag, Sequence Number, Acknowledgment) apply to each individual LPP message segment, independently of the value of the IE *SegmentationInfo*.



Figure 4.3.5-1: LPP Message Segmentation procedure

1. Endpoint A sends an LPP message to Endpoint B for a particular location session and includes the IE *SegmentationInfo* set to *moreMessagesOnTheWay* to indicate that this is one of many LPP message segments used to deliver the entire LPP message body.

2 Endpoint A may send one or more additional LPP messages to Endpoint B with the IE *SegmentationInfo* set to *moreMessagesOnTheWay* to continue delivering the segmented LPP message*.*

3. Endpoint A sends the final LPP message segment to Endpoint B and includes the IE *SegmentationInfo* set to *noMoreMessages* to indicate that this is the final LPP message segment. Endpoint B assumes that the complete LPP message body has been received.

# 5 LPP Procedures

## 5.1 Procedures related to capability transfer

The purpose of the procedures that are grouped together in this clause is to enable the transfer of capabilities from the target device to the server. Capabilities in this context refer to positioning and protocol capabilities related to LPP and the positioning methods supported by LPP.

These procedures instantiate the Capability Transfer transaction from TS 36.305 [2] and TS 38.305 [40].

### 5.1.1 Capability Transfer procedure

The Capability Transfer procedure is shown in Figure 5.1.1-1.



Figure 5.1.1-1: LPP Capability Transfer procedure

1. The server sends a *RequestCapabilities* message to the target. The server may indicate the types of capability needed.

2. The target responds with a *ProvideCapabilities* message to the server. The capabilities shall correspond to any capability types specified in step 1. This message shall include the *endTransaction* IE set to TRUE.

### 5.1.2 Capability Indication procedure

The Capability Indication procedure allows the target to provide unsolicited capabilities to the server and is shown in Figure 5.1.2-1.



Figure 5.1.2-1: LPP Capability Indication procedure

1. The target sends a *ProvideCapabilities* message to the server. This message shall include the *endTransaction* IE set to TRUE.

### 5.1.3 Reception of LPP Request Capabilities

Upon receiving a *RequestCapabilities* message, the target device shall generate a *ProvideCapabilities* message as a response.

The target device shall:

1> for each positioning method for which a request for capabilities is included in the message:

2> if the target device supports this positioning method:

3> include the capabilities of the device for that supported positioning method in the response message;

1> set the IE *LPP-TransactionID* in the response message to the same value as the IE *LPP-TransactionID* in the received message;

1> deliver the response message to lower layers for transmission.

### 5.1.4 Transmission of LPP Provide Capabilities

When triggered to transmit a *ProvideCapabilities* message, the target device shall:

1> for each positioning method whose capabilities are to be indicated:

2> set the corresponding IE to include the device's capabilities;

2> if OTDOA capabilities are to be indicated:

3> include the IE *supportedBandListEUTRA*;

1> deliver the response to lower layers for transmission.

## 5.2 Procedures related to Assistance Data Transfer

The purpose of the procedures in this clause is to enable the target to request assistance data from the server to assist in positioning, and to enable the server to transfer assistance data to the target in the absence of a request.

These procedures instantiate the Assistance Data Transfer transaction from TS 36.305 [2] and TS 38.305 [40].

### 5.2.1 Assistance Data Transfer procedure

The Assistance Data Transfer procedure is shown in Figure 5.2.1-1.



Figure 5.2.1-1: LPP Assistance data transfer procedure

1. The target sends a *RequestAssistanceData* message to the server.

2. The server responds with a *ProvideAssistanceData* message to the target containing assistance data. The transferred assistance data should match or be a subset of the assistance data requested in step 1. The server may also provide any not requested information that it considers useful to the target. If step 3 does not occur, this message shall set the *endTransaction* IE to TRUE.

3. The server may transmit one or more additional *ProvideAssistanceData* messages to the target containing further assistance data. The transferred assistance data should match or be a subset of the assistance data requested in step 1. The server may also provide any not requested information that it considers useful to the target. The last message shall include the *endTransaction* IE set to TRUE.

### 5.2.1a Periodic Assistance Data Transfer procedure

The Periodic Assistance Data Transfer procedure is shown in Figure 5.2.1a-1. This procedure enables a target to request a server to send assistance data periodically.

NOTE 1: In this version of the specification, periodic assistance data transfer is supported for HA GNSS (e.g., RTK) and NR DL-TDOA positioning only.



Figure 5.2.1a-1: LPP Periodic Assistance data transfer procedure

1. The target sends a *RequestAssistanceData* message to the server using some available *transactionID* T1. The message contains a *periodicSessionID* S (different to any other *periodicSessionID* currently in use between the target and server) in the IE *CommonIEsRequestAssistanceData.* The message also includes a positioning method specific assistance data request element (e.g., IE *A-GNSS-RequestAssistanceData*) identifying the type of assistance data being requested together with desired periodicity conditions for sending it and a duration for ending the assistance data transfer (e.g., in IE *GNSS-PeriodicAssistDataReq*).

2. The server responds with a *ProvideAssistanceData* message to the target. The message uses the *transactionID* T1 in step 1 and indicates the end of this transaction. The message contains the *periodicSessionID* S in IE *CommonIEsProvideAssistanceData.* If the request can be supported, the message contains the control parameters in the positioning method specific assistance data (e.g., IE *A-GNSS-ProvideAssistanceData)* which may confirm or redefine the type of assistance data or periodicity parameters requested at step 1 (e.g., in IE *GNSS‑PeriodicAssistData*). If the target requested non-periodic assistance data in addition to the periodic assistance data in step 1, the *ProvideAssistanceData* message may also include the non-periodic assistance data in this step 2 (but not any periodic assistance data).  
If the request cannot be supported (fully or partly), an error reason is provided in the positioning method specific IE (e.g., IE *A‑GNSS‑Error*). If the request cannot even partly be supported remaining steps are then not performed.

NOTE 2: The target device infers from an absence of the *periodicSessionID* that the location server does not support periodic assistance data delivery. In that case, the target device does not expect the Data Transaction (Steps 3-7).

3. When the first periodic message is available, the server sends an unsolicited *ProvideAssistanceData* message to the target containing the *periodicSessionID* S and the periodic assistance data confirmed in step 2. The message uses some available *transactionID* T2 that may be different to T1.

NOTE 3: The positioning method specific control parameters (e.g., IE *GNSS-PeriodicAssistData*) are not included in the data transaction.

4. The server may continue to send further *ProvideAssistanceData* messages to the target containing the periodic assistance data confirmed or redefined in step 2 when each additional periodicity condition occurs.

NOTE 4: The target device expects a *ProvideAssistanceData* messages at the in Step 2 confirmed interval(s). If some or all of the assistance data is not available at each periodic interval, an error indication is provided in the positioning method specific IE (e.g., IE *A‑GNSS‑Error*).

5. If the target requires the session to end, the target sends an *Abort* message to the server for transaction T2 that may optionally include an *abortCause*. Remaining steps are then omitted.

6. If the server requires the session to end, the server sends an *Abort* message to the target for transaction T2 that may optionally include an *abortCause*. Remaining steps are then omitted.

7. When the duration or other conditions for ending the periodic assistance data transfer occur, the last *ProvideAssistanceData* message transferred indicates the end of transaction T2.

### 5.2.1b Periodic Assistance Data Transfer with Update procedure



Figure 5.2.1b-1: LPP Periodic Assistance data transfer with update procedure

1. Steps 1-2 and optionally steps 3-4 are performed for the Periodic Assistance Data Transfer procedure in clause 5.2.1a with the following exceptions:

- The *RequestAssistanceData* message in step 1 indicates the update capabilities of the target device.

- The *ProvideAssistanceData* message in step 2 indicates the update capabilities of the target device which are supported by the server.

2. If the target device changes its primary cell and if the update capabilities of the target device supported by the server in step 1 include update of a primary cell ID, the target device sends a *RequestAssistanceData* message to the server using some available *transactionID* T3, which is different from T2 (previously used in step 2). The message contains the *periodicSessionID* S (previously used in step 1) and the new primary cell ID in the IE *CommonIEsRequestAssistanceData.*

3. The server responds with a *ProvideAssistanceData* message to the target. The message uses the *transactionID* T3 in step 2 and indicates the end of this transaction. The message contains the *periodicSessionID* S in IE *CommonIEsProvideAssistanceData.* Steps 2-3 are repeated each time the target device changes its primary cell.

4. Steps 4-7 are performed for the Periodic Assistance Data Transfer procedure in clause 5.2.1a.

### 5.2.2 Assistance Data Delivery procedure

The Assistance Data Delivery procedure allows the server to provide unsolicited assistance data to the target and is shown in Figure 5.2.2-1.



Figure 5.2.2-1: LPP Assistance data transfer procedure

1. The server sends a *ProvideAssistanceData* message to the target containing assistance data. If step 2 does not occur, this message shall set the *endTransaction* IE to TRUE.

2. The server may transmit one or more additional *ProvideAssistanceData* messages to the target containing additional assistance data. The last message shall include the *endTransaction* IE set to TRUE.

### 5.2.2a Periodic Assistance Data Delivery procedure

The Periodic Assistance Data Delivery procedure allows the server to provide unsolicited periodic assistance data to the target and is shown in Figure 5.2.2a-1.

NOTE 1: In this version of the specification, periodic assistance data delivery is supported for HA GNSS (e.g., RTK) and NR DL-TDOA positioning only.



Figure 5.2.2a-1: LPP Periodic Assistance data delivery procedure

1. The server sends a *ProvideAssistanceData* message to the target using some available *transactionID* T1 and indicates the end of this transaction. The message contains a *periodicSessionID* S (different to any other *periodicSessionID* currently in use between the server and target) in the IE *CommonIEsProvideAssistanceData.* The message includes positioning method specific assistance data control parameters (e.g., in IE *A‑GNSS‑ProvideAssistanceData*) identifying the type of periodic assistance data being delivered together with periodicity conditions for sending it and a duration for ending the assistance data delivery (e.g., in IE *GNSS‑PeriodicAssistData*). The *ProvideAssistanceData* message may also include non-periodic assistance data (but not any periodic assistance data).

2. When the first periodic message is available, the server sends an unsolicited *ProvideAssistanceData* message to the target containing the *periodicSessionID* S and the periodic assistance data announced in step 1. The message uses some available *transactionID* T2 that may be different to T1.

NOTE 2: The positioning method specific control parameters (e.g., IE *GNSS-PeriodicAssistData*) are not included in the data transaction.

3. The server may continue to send further *ProvideAssistanceData* messages to the target containing the periodic assistance data announced in step 2 when each additional periodicity condition occurs.

NOTE3: The target device expects a *ProvideAssistanceData* messages at the in Step 2 announced interval(s). If some or all of the assistance data is not available at each periodic interval, an error indication is provided in the positioning method specific IE (e.g., IE *A‑GNSS‑Error*).

4. If the target requires the session to end, the target sends an *Abort* message to the server for transaction T2 that may optionally include an *abortCause*. Remaining steps are then omitted.

5. If the server requires the session to end, the server sends an *Abort* message to the target for transaction T2 that may optionally include an *abortCause*. Remaining steps are then omitted.

6. When the duration or other conditions for ending the periodic assistance data transfer occur, the last *ProvideAssistanceData* message transferred indicates the end of transaction T2.

### 5.2.3 Transmission of LPP Request Assistance Data

When triggered to transmit a *RequestAssistanceData* message, the target device shall:

1> set the IEs for the positioning-method-specific request for assistance data to request the data indicated by upper layers.

### 5.2.4 Reception of LPP Provide Assistance Data

Upon receiving a *ProvideAssistanceData* message, the target device shall:

1> for each positioning method contained in the message:

2> deliver the related assistance data to upper layers.

## 5.3 Procedures related to Location Information Transfer

The purpose of the procedures in this clause is to enable the server to request location measurement data and/or a location estimate from the target, and to enable the target to transfer location measurement data and/or a location estimate to a server in the absence of a request.

These procedures instantiate the Location Information Transfer transaction in TS 36.305 [2] and TS 38.305 [40].

NOTE: The service layer (e.g. NAS or OMA SUPL ULP) would be used to transfer information associated with a location request from a target to a server (MO-LR).

### 5.3.1 Location Information Transfer procedure

The Location Information Transfer procedure is shown in Figure 5.3.1-1.



Figure 5.3.1-1: LPP Location Information transfer procedure

1. The server sends a *RequestLocationInformation* message to the target to request location information, indicating the type of location information needed and potentially the associated QoS.

2. The target sends a *ProvideLocationInformation* message to the server to transfer location information. The location information transferred should match or be a subset of the location information requested in step 1 unless the server explicitly allows additional location information. If step 3 does not occur, this message shall set the *endTransaction* IE to TRUE.

3. If requested in step 1, the target sends additional *ProvideLocationInformation* messages to the server to transfer location information. The location information transferred should match or be a subset of the location information requested in step 1 unless the server explicitly allows additional location information. The last message shall include the *endTransaction* IE set to TRUE.

### 5.3.2 Location Information Delivery procedure

The Location Information Delivery allows the target to provide unsolicited location information to the server. The procedure is shown in Figure 5.3.2-1.



Figure 5.3.2-1: LPP Location Information Delivery procedure

1. The target sends a *ProvideLocationInformation* message to the server to transfer location information. If step 2 does not occur, this message shall set the *endTransaction* IE to TRUE.

2. The target may send one or more additional *ProvideLocationInformation* messages to the server containing additional location information data. The last message shall include the *endTransaction* IE set to TRUE.

### 5.3.3 Reception of Request Location Information

Upon receiving a *RequestLocationInformation* message, the target device shall:

1> if the requested information is compatible with the target device capabilities and configuration:

2> include the requested information in a *ProvideLocationInformation* message;

2> set the IE *LPP-TransactionID* in the response to the same value as the IE *LPP-TransactionID* in the received message;

2> deliver the *ProvideLocationInformation* message to lower layers for transmission.

1> otherwise:

2> if one or more positioning methods are included that the target device does not support:

3> continue to process the message as if it contained only information for the supported positioning methods;

3> handle the signaling content of the unsupported positioning methods by LPP error detection as in 5.4.3.

### 5.3.4 Transmission of Provide Location Information

When triggered to transmit *ProvideLocationInformation* message, the target device shall:

1> for each positioning method contained in the message:

2> set the corresponding IE to include the available location information;

1> deliver the response to lower layers for transmission.

## 5.4 Error Handling Procedures

### 5.4.1 General

This clause describes how a receiving entity (target device or location server) behaves in cases when it receives erroneous or unexpected data or detects that certain data are missing.

### 5.4.2 Procedures related to Error Indication

Figure 5.4.2-1 shows the Error indication procedure.



Figure 5.4.2-1: LPP Error Indication procedure

1. Endpoint A sends an LPP message to Endpoint B.

2. Endpoint B determines that the LPP message in step 1 contains an error. Endpoint B returns an *Error* message to Endpoint A indicating the error or errors and discards the message in step 1. If Endpoint B is able to determine that the erroneous LPP message in step 1 is an LPP Error or Abort Message, Endpoint B discards the message in step 1 without returning an *Error* message to Endpoint A.

### 5.4.3 LPP Error Detection

Upon receiving any LPP message, the receiving entity shall attempt to decode the message and verify the presence of any errors and:

1> if decoding errors are encountered:

2> if the receiver can not determine that the received message is an LPP *Error* or *Abort* message:

3> return an LPP *Error* message to the sender and include the received *LPP-TransactionID*, if this was decoded, and type of error;

3> if the receiver can determine the session and the *LPP-TransactionID* and the received message includes the IE *SegmentationInfo* and the receiver has previously stored message segments for this session and *LPP-TransactionID*:

4> discard all stored LPP message segments for this session and *LPP-TransactionID*;

3> discard the received message and stop the error detection procedure;

1> if the message is a duplicate of a previously received message:

2> discard the message and stop the error detection procedure;

1> if the *LPP-TransactionID* matches the *LPP-TransactionID* for a procedure that is still ongoing for the same session and the message type is invalid for the current state of the procedure:

2> abort the ongoing procedure;

2> return an LPP *Error* message to the sender and include the received transaction ID and type of error;

2> if the message includes the IE *SegmentationInfo* and the receiver has previously stored message segments for this session and *LPP-TransactionID*:

3> discard all stored LPP message segments for this session and *LPP-TransactionID;*

2> discard the message and stop the error detection procedure;

1> if the message includes the IE *SegmentationInfo*:

2> if the receiver has previously stored LPP message segments for this session and *LPP-TransactionID*:

3> if the received message type is different to the stored message type:

4> return an LPP *Error* message to the sender and include the received transaction ID and type of error;

4> discard the message and all stored LPP message segments for this session and *LPP-TransactionID* and stop the error detection procedure;

2> if the IE *SegmentationInfo* has the value *moreMessagesOnTheWay*:

3> store the received message;

NOTE: As an implementation option, the receiver of an LPP Provide Assistance Data or LPP Provide Location Information message may process the received message segment instead of storing the message.

2> if the IE *SegmentationInfo* has the value *noMoreMessages*:

3> continue error detection for the received message and any stored LPP message segments for this session and *LPP-TransactionID*;

1> if the message type is an LPP *RequestCapabilities* and some of the requested information is not supported:

2> return any information that can be provided in a normal response.

1> if the message type is an LPP *RequestAssistanceData* or *RequestLocationInformation* and some or all of the requested information is not supported:

2> return any information that can be provided in a normal response, which includes indications on other information that is not supported.

### 5.4.4 Reception of an LPP Error Message

Upon receiving an *Error* message, a device shall:

1> abort any ongoing procedure associated with the *LPP-TransactionID* if included in the received message.

The device may:

1> restart the aborted procedure taking into consideration the returned error information.

## 5.5 Abort Procedure

### 5.5.1 General

The purpose of the abort procedure is to allow the target device or location server to abort an ongoing procedure due to some unexpected event (e.g., cancellation of a location request by an LCS client). It can also be used to stop an ongoing procedure (e.g., periodic location reporting from the target device).

### 5.5.2 Procedures related to Abort

Figure 5.5.2-1 shows the Abort procedure.



Figure 5.5.2-1: LPP Abort procedure

1. A procedure P is ongoing between endpoints A and B.

2. Endpoint A determines that the procedure must be aborted and sends an *Abort* message to Endpoint B carrying the transaction ID for procedure P. Endpoint B aborts procedure P.

### 5.5.3 Reception of an LPP Abort Message

Upon receiving an *Abort* message, a device shall:

1> abort any ongoing procedure associated with the transaction ID indicated in the message.

# 6 Information Element Abstract Syntax Definition

## 6.1 General

The contents of each LPP message is specified in clause 6.2 using ASN.1 to specify the message syntax and using tables when needed to provide further detailed information about the fields specified in the message syntax.

The ASN.1 in this clause uses the same format and coding conventions as described in Annex A of TS 36.331 [12].

Transfer syntax for LPP messages is derived from their ASN.1 definitions by use of Basic Packed Encoding Rules (BASIC-PER), Unaligned Variant, as specified in ITU-T Rec. X.691 [22]. The encoded LPP message always contains a multiple of 8 bits.

Transfer syntax for LPP IEs is derived from their ASN.1 definitions by use of Basic Packed Encoding Rules (BASIC-PER), Unaligned Variant, as specified in ITU-T Rec. X.691 [22]. The encoded LPP IE always contains a multiple of 8 bits. This applies when a single LPP IE is encoded as the basic production, i.e. for other purposes than encoding the LPP IE within an LPP message.

The need for fields to be present in a message or an abstract type, i.e., the ASN.1 fields that are specified as OPTIONAL in the abstract notation (ASN.1), is specified by means of comment text tags attached to the OPTIONAL statement in the abstract syntax. The meaning of each tag is specified in table 6.1-1. The use of these tags in the uplink (target to server) direction does not impose any requirements on the server.

Table 6.1-1: Meaning of abbreviations used to specify the need for fields to be present

| Abbreviation | Meaning |
| --- | --- |
| Cond *conditionTag* | *Conditionally present*  A field for which the need is specified by means of conditions. For each *conditionTag*, the need is specified in a tabular form following the ASN.1 segment. In case, according to the conditions, a field is not present, the target takes no action and where applicable shall continue to use the existing value (and/or the associated functionality) unless explicitly stated otherwise in the description of the field itself. |
| Need OP | *Optionally present*  A field that is optional to signal. For downlink messages, the target is not required to take any special action on absence of the field beyond what is specified in the procedural text or the field description table following the ASN.1 segment. The target behaviour on absence should be captured either in the procedural text or in the field description. |
| Need ON | *Optionally present, No action*  A field that is optional to signal. If the message is received by the target, and in case the field is absent, the target takes no action and where applicable shall continue to use the existing value (and/or the associated functionality). |
| Need OR | *Optionally present, Release*  A field that is optional to signal. If the message is received by the target, and in case the field is absent, the target shall discontinue/ stop using/ delete any existing value (and/ or the associated functionality). |

When specifying information elements which are to be represented by BIT STRINGs, if not otherwise specifically stated in the field description of the concerned IE or elsewhere, the following principle applies with regards to the ordering of bits:

- The first bit (leftmost bit) contains the most significant bit (MSB);

- the last bit (rightmost bit) contains the least significant bit (LSB).

## 6.2 LPP PDU Structure

#### *– LPP-PDU-Definitions*

This ASN.1 segment is the start of the LPP PDU definitions.

-- ASN1START

LPP-PDU-Definitions

DEFINITIONS AUTOMATIC TAGS ::=

BEGIN

-- ASN1STOP

#### *– LPP-Message*

The *LPP-Message* provides the complete set of information for an invocation or response pertaining to an LPP transaction.

-- ASN1START

LPP-Message ::= SEQUENCE {

transactionID LPP-TransactionID OPTIONAL, -- Need ON

endTransaction BOOLEAN,

sequenceNumber SequenceNumber OPTIONAL, -- Need ON

acknowledgement Acknowledgement OPTIONAL, -- Need ON

lpp-MessageBody LPP-MessageBody OPTIONAL -- Need ON

}

SequenceNumber ::= INTEGER (0..255)

Acknowledgement ::= SEQUENCE {

ackRequested BOOLEAN,

ackIndicator SequenceNumber OPTIONAL

}

-- ASN1STOP

| ***LPP-Message* field descriptions** |
| --- |
| ***transactionID***  This field is omitted if an *lpp-MessageBody* is not present (i.e. in an LPP message sent only to acknowledge a previously received message) or if it is not available to the transmitting entity (e.g., in an *LPP-Error* message triggered by a message that could not be parsed). If present, this field shall be ignored at a receiver in an LPP message for which the *lpp-MessageBody* is not present. | |
| ***endTransaction***  This field indicates whether an LPP message is the last message carrying an *lpp-MessageBody* in a transaction (TRUE) or not last (FALSE). When LPP message segmentation is used, only the final LPP message segment may indicate the end of the transaction. | |
| ***sequenceNumber***  This field may be included when LPP operates over the control plane and an *lpp-MessageBody* is included but shall be omitted otherwise. | |
| ***acknowledgement***  This field is included in an LPP acknowledgement and in any LPP message requesting an acknowledgement when LPP operates over the control plane and is omitted otherwise. | |
| ***ackRequested***  This field indicates whether an LPP acknowledgement is requested (TRUE) or not (FALSE). A value of TRUE may only be included when an *lpp-MessageBody* is included. | |
| ***ackIndicator***  This field indicates the sequence number of the message being acknowledged. | |
| ***lpp-MessageBody***  This field may be omitted in the case the message is sent only to acknowledge a previously received message. |

#### *– LPP-MessageBody*

The *LPP-MessageBody* identifies the type of an LPP message and contains all LPP information specifically associated with that type.

-- ASN1START

LPP-MessageBody ::= CHOICE {

c1 CHOICE {

requestCapabilities RequestCapabilities,

provideCapabilities ProvideCapabilities,

requestAssistanceData RequestAssistanceData,

provideAssistanceData ProvideAssistanceData,

requestLocationInformation RequestLocationInformation,

provideLocationInformation ProvideLocationInformation,

abort Abort,

error Error,

spare7 NULL, spare6 NULL, spare5 NULL, spare4 NULL,

spare3 NULL, spare2 NULL, spare1 NULL, spare0 NULL

},

messageClassExtension SEQUENCE {}

}

-- ASN1STOP

#### *– LPP-TransactionID*

The *LPP-TransactionID* identifies a particular LPP transaction and the initiator of the transaction.

-- ASN1START

LPP-TransactionID ::= SEQUENCE {

initiator Initiator,

transactionNumber TransactionNumber,

...

}

Initiator ::= ENUMERATED {

locationServer,

targetDevice,

...

}

TransactionNumber ::= INTEGER (0..255)

-- ASN1STOP

## 6.3 Message Body IEs

#### – *RequestCapabilities*

The *RequestCapabilities* message body in a LPP message is used by the location server to request the target device capability information for LPP and the supported individual positioning methods.

-- ASN1START

RequestCapabilities ::= SEQUENCE {

criticalExtensions CHOICE {

c1 CHOICE {

requestCapabilities-r9 RequestCapabilities-r9-IEs,

spare3 NULL, spare2 NULL, spare1 NULL

},

criticalExtensionsFuture SEQUENCE {}

}

}

RequestCapabilities-r9-IEs ::= SEQUENCE {

commonIEsRequestCapabilities CommonIEsRequestCapabilities OPTIONAL, -- Need ON

a-gnss-RequestCapabilities A-GNSS-RequestCapabilities OPTIONAL, -- Need ON

otdoa-RequestCapabilities OTDOA-RequestCapabilities OPTIONAL, -- Need ON

ecid-RequestCapabilities ECID-RequestCapabilities OPTIONAL, -- Need ON

epdu-RequestCapabilities EPDU-Sequence OPTIONAL, -- Need ON

...,

[[ sensor-RequestCapabilities-r13 Sensor-RequestCapabilities-r13 OPTIONAL, -- Need ON

tbs-RequestCapabilities-r13 TBS-RequestCapabilities-r13 OPTIONAL, -- Need ON

wlan-RequestCapabilities-r13 WLAN-RequestCapabilities-r13 OPTIONAL, -- Need ON

bt-RequestCapabilities-r13 BT-RequestCapabilities-r13 OPTIONAL -- Need ON

]],

[[ nr-ECID-RequestCapabilities-r16 NR-ECID-RequestCapabilities-r16 OPTIONAL, -- Need ON

nr-Multi-RTT-RequestCapabilities-r16

NR-Multi-RTT-RequestCapabilities-r16

OPTIONAL, -- Need ON

nr-DL-AoD-RequestCapabilities-r16

NR-DL-AoD-RequestCapabilities-r16 OPTIONAL, -- Need ON

nr-DL-TDOA-RequestCapabilities-r16

NR-DL-TDOA-RequestCapabilities-r16 OPTIONAL, -- Need ON

nr-UL-RequestCapabilities-r16 NR-UL-RequestCapabilities-r16 OPTIONAL -- Need ON

]],

[[

nr-AI-ML-PositioningRequestCapabilities-r19

NR-AI-ML-PositioningRequestCapabilities-r19

OPTIONAL -- Need ON

]]

}

-- ASN1STOP

#### – *ProvideCapabilities*

The *ProvideCapabilities* message body in a LPP message indicates the LPP capabilities of the target device to the location server.

-- ASN1START

ProvideCapabilities ::= SEQUENCE {

criticalExtensions CHOICE {

c1 CHOICE {

provideCapabilities-r9 ProvideCapabilities-r9-IEs,

spare3 NULL, spare2 NULL, spare1 NULL

},

criticalExtensionsFuture SEQUENCE {}

}

}

ProvideCapabilities-r9-IEs ::= SEQUENCE {

commonIEsProvideCapabilities CommonIEsProvideCapabilities OPTIONAL,

a-gnss-ProvideCapabilities A-GNSS-ProvideCapabilities OPTIONAL,

otdoa-ProvideCapabilities OTDOA-ProvideCapabilities OPTIONAL,

ecid-ProvideCapabilities ECID-ProvideCapabilities OPTIONAL,

epdu-ProvideCapabilities EPDU-Sequence OPTIONAL,

...,

[[ sensor-ProvideCapabilities-r13 Sensor-ProvideCapabilities-r13 OPTIONAL,

tbs-ProvideCapabilities-r13 TBS-ProvideCapabilities-r13 OPTIONAL,

wlan-ProvideCapabilities-r13 WLAN-ProvideCapabilities-r13 OPTIONAL,

bt-ProvideCapabilities-r13 BT-ProvideCapabilities-r13 OPTIONAL

]],

[[ nr-ECID-ProvideCapabilities-r16 NR-ECID-ProvideCapabilities-r16 OPTIONAL,

nr-Multi-RTT-ProvideCapabilities-r16

NR-Multi-RTT-ProvideCapabilities-r16 OPTIONAL,

nr-DL-AoD-ProvideCapabilities-r16

NR-DL-AoD-ProvideCapabilities-r16 OPTIONAL,

nr-DL-TDOA-ProvideCapabilities-r16

NR-DL-TDOA-ProvideCapabilities-r16 OPTIONAL,

nr-UL-ProvideCapabilities-r16 NR-UL-ProvideCapabilities-r16 OPTIONAL

]],

[[

nr-AI-ML-PositioningProvideCapabilities-r19

NR-AI-ML-PositioningProvideCapabilities-r19

OPTIONAL

]]

}

-- ASN1STOP

#### – *RequestAssistanceData*

The *RequestAssistanceData* message body in a LPP message is used by the target device to request assistance data from the location server.

-- ASN1START

RequestAssistanceData ::= SEQUENCE {

criticalExtensions CHOICE {

c1 CHOICE {

requestAssistanceData-r9 RequestAssistanceData-r9-IEs,

spare3 NULL, spare2 NULL, spare1 NULL

},

criticalExtensionsFuture SEQUENCE {}

}

}

RequestAssistanceData-r9-IEs ::= SEQUENCE {

commonIEsRequestAssistanceData CommonIEsRequestAssistanceData OPTIONAL,

a-gnss-RequestAssistanceData A-GNSS-RequestAssistanceData OPTIONAL,

otdoa-RequestAssistanceData OTDOA-RequestAssistanceData OPTIONAL,

epdu-RequestAssistanceData EPDU-Sequence OPTIONAL,

...,

[[ sensor-RequestAssistanceData-r14

Sensor-RequestAssistanceData-r14 OPTIONAL,

tbs-RequestAssistanceData-r14 TBS-RequestAssistanceData-r14 OPTIONAL,

wlan-RequestAssistanceData-r14 WLAN-RequestAssistanceData-r14 OPTIONAL

]],

[[ nr-Multi-RTT-RequestAssistanceData-r16 NR-Multi-RTT-RequestAssistanceData-r16 OPTIONAL,

nr-DL-AoD-RequestAssistanceData-r16 NR-DL-AoD-RequestAssistanceData-r16 OPTIONAL,

nr-DL-TDOA-RequestAssistanceData-r16 NR-DL-TDOA-RequestAssistanceData-r16 OPTIONAL

]],

[[

bt-RequestAssistanceData-r18 BT-RequestAssistanceData-r18 OPTIONAL

]],

[[

nr-AI-ML-PositioningRequestAssistanceData-r19

NR-AI-ML-PositioningRequestAssistanceData-r19

OPTIONAL

]]

}

-- ASN1STOP

#### – *ProvideAssistanceData*

The *ProvideAssistanceData* message body in a LPP message is used by the location server to provide assistance data to the target device either in response to a request from the target device or in an unsolicited manner.

-- ASN1START

ProvideAssistanceData ::= SEQUENCE {

criticalExtensions CHOICE {

c1 CHOICE {

provideAssistanceData-r9 ProvideAssistanceData-r9-IEs,

spare3 NULL, spare2 NULL, spare1 NULL

},

criticalExtensionsFuture SEQUENCE {}

}

}

ProvideAssistanceData-r9-IEs ::= SEQUENCE {

commonIEsProvideAssistanceData CommonIEsProvideAssistanceData OPTIONAL, -- Need ON

a-gnss-ProvideAssistanceData A-GNSS-ProvideAssistanceData OPTIONAL, -- Need ON

otdoa-ProvideAssistanceData OTDOA-ProvideAssistanceData OPTIONAL, -- Need ON

epdu-Provide-Assistance-Data EPDU-Sequence OPTIONAL, -- Need ON

...,

[[

sensor-ProvideAssistanceData-r14 Sensor-ProvideAssistanceData-r14 OPTIONAL, -- Need ON

tbs-ProvideAssistanceData-r14 TBS-ProvideAssistanceData-r14 OPTIONAL, -- Need ON

wlan-ProvideAssistanceData-r14 WLAN-ProvideAssistanceData-r14 OPTIONAL -- Need ON

]],

[[ nr-Multi-RTT-ProvideAssistanceData-r16

NR-Multi-RTT-ProvideAssistanceData-r16

OPTIONAL, -- Need ON

nr-DL-AoD-ProvideAssistanceData-r16

NR-DL-AoD-ProvideAssistanceData-r16 OPTIONAL, -- Need ON

nr-DL-TDOA-ProvideAssistanceData-r16

NR-DL-TDOA-ProvideAssistanceData-r16

OPTIONAL -- Need ON

]],

[[

bt-ProvideAssistanceData-r18 BT-ProvideAssistanceData-r18 OPTIONAL -- Need ON

]],

[[

nr-AI-ML-PositioningProvideAssistanceData-r19

NR-AI-ML-PositioningProvideAssistanceData-r19

OPTIONAL -- Need ON

]]

}

-- ASN1STOP

#### – *RequestLocationInformation*

The *RequestLocationInformation* message body in a LPP message is used by the location server to request positioning measurements or a position estimate from the target device.

-- ASN1START

RequestLocationInformation ::= SEQUENCE {

criticalExtensions CHOICE {

c1 CHOICE {

requestLocationInformation-r9 RequestLocationInformation-r9-IEs,

spare3 NULL, spare2 NULL, spare1 NULL

},

criticalExtensionsFuture SEQUENCE {}

}

}

RequestLocationInformation-r9-IEs ::= SEQUENCE {

commonIEsRequestLocationInformation

CommonIEsRequestLocationInformation OPTIONAL, -- Need ON

a-gnss-RequestLocationInformation A-GNSS-RequestLocationInformation OPTIONAL, -- Need ON

otdoa-RequestLocationInformation OTDOA-RequestLocationInformation OPTIONAL, -- Need ON

ecid-RequestLocationInformation ECID-RequestLocationInformation OPTIONAL, -- Need ON

epdu-RequestLocationInformation EPDU-Sequence OPTIONAL, -- Need ON

...,

[[

sensor-RequestLocationInformation-r13

Sensor-RequestLocationInformation-r13

OPTIONAL, -- Need ON

tbs-RequestLocationInformation-r13 TBS-RequestLocationInformation-r13 OPTIONAL, -- Need ON

wlan-RequestLocationInformation-r13 WLAN-RequestLocationInformation-r13 OPTIONAL, -- Need ON

bt-RequestLocationInformation-r13 BT-RequestLocationInformation-r13 OPTIONAL -- Need ON

]],

[[ nr-ECID-RequestLocationInformation-r16

NR-ECID-RequestLocationInformation-r16

OPTIONAL, -- Need ON

nr-Multi-RTT-RequestLocationInformation-r16

NR-Multi-RTT-RequestLocationInformation-r16

OPTIONAL, -- Need ON

nr-DL-AoD-RequestLocationInformation-r16

NR-DL-AoD-RequestLocationInformation-r16

OPTIONAL, -- Need ON

nr-DL-TDOA-RequestLocationInformation-r16

NR-DL-TDOA-RequestLocationInformation-r16

OPTIONAL -- Need ON

]],

[[

nr-AI-ML-PositioningRequestLocationInformation-r19

NR-AI-ML-PositioningRequestLocationInformation-r19

OPTIONAL -- Need ON

]]

}

-- ASN1STOP

| *RequestLocationInformation* field descriptions |
| --- |
| ***commonIEsRequestLocationInformation***  This field specifies the location information type requested by the location server and optionally other configuration information associated with the requested location information. This field should always be included in this version of the protocol. |

#### – *ProvideLocationInformation*

The *ProvideLocationInformation* message body in a LPP message is used by the target device to provide positioning measurements or position estimates to the location server.

-- ASN1START

ProvideLocationInformation ::= SEQUENCE {

criticalExtensions CHOICE {

c1 CHOICE {

provideLocationInformation-r9 ProvideLocationInformation-r9-IEs,

spare3 NULL, spare2 NULL, spare1 NULL

},

criticalExtensionsFuture SEQUENCE {}

}

}

ProvideLocationInformation-r9-IEs ::= SEQUENCE {

commonIEsProvideLocationInformation

CommonIEsProvideLocationInformation OPTIONAL,

a-gnss-ProvideLocationInformation A-GNSS-ProvideLocationInformation OPTIONAL,

otdoa-ProvideLocationInformation OTDOA-ProvideLocationInformation OPTIONAL,

ecid-ProvideLocationInformation ECID-ProvideLocationInformation OPTIONAL,

epdu-ProvideLocationInformation EPDU-Sequence OPTIONAL,

...,

[[

sensor-ProvideLocationInformation-r13

Sensor-ProvideLocationInformation-r13

OPTIONAL,

tbs-ProvideLocationInformation-r13 TBS-ProvideLocationInformation-r13 OPTIONAL,

wlan-ProvideLocationInformation-r13 WLAN-ProvideLocationInformation-r13 OPTIONAL,

bt-ProvideLocationInformation-r13 BT-ProvideLocationInformation-r13 OPTIONAL

]],

[[ nr-ECID-ProvideLocationInformation-r16

NR-ECID-ProvideLocationInformation-r16 OPTIONAL,

nr-Multi-RTT-ProvideLocationInformation-r16

NR-Multi-RTT-ProvideLocationInformation-r16 OPTIONAL,

nr-DL-AoD-ProvideLocationInformation-r16

NR-DL-AoD-ProvideLocationInformation-r16 OPTIONAL,

nr-DL-TDOA-ProvideLocationInformation-r16

NR-DL-TDOA-ProvideLocationInformation-r16 OPTIONAL

]],

[[

nr-AI-ML-PositioningProvideLocationInformation-r19

NR-AI-ML-PositioningProvideLocationInformation-r19

OPTIONAL

]]

}

-- ASN1STOP

#### *– Abort*

The *Abort* message body in a LPP message carries a request to abort an ongoing LPP procedure.

-- ASN1START

Abort ::= SEQUENCE {

criticalExtensions CHOICE {

c1 CHOICE {

abort-r9 Abort-r9-IEs,

spare3 NULL, spare2 NULL, spare1 NULL

},

criticalExtensionsFuture SEQUENCE {}

}

}

Abort-r9-IEs ::= SEQUENCE {

commonIEsAbort CommonIEsAbort OPTIONAL, -- Need ON

...,

epdu-Abort EPDU-Sequence OPTIONAL -- Need ON

}

-- ASN1STOP

#### *– Error*

The *Error* message body in a LPP message carries information concerning a LPP message that was received with errors.

-- ASN1START

Error ::= CHOICE {

error-r9 Error-r9-IEs,

criticalExtensionsFuture SEQUENCE {}

}

Error-r9-IEs ::= SEQUENCE {

commonIEsError CommonIEsError OPTIONAL, -- Need ON

...,

epdu-Error EPDU-Sequence OPTIONAL -- Need ON

}

-- ASN1STOP

## 6.4 Common IEs

Common IEs comprise IEs that are applicable to more than one LPP positioning method.

### 6.4.1 Common Lower-Level IEs

#### – *AccessTypes*

The IE *AccessTypes* is used to indicate several cellular access types using a bit map.

-- ASN1START

AccessTypes ::= SEQUENCE {

accessTypes BIT STRING { eutra (0),

utra (1),

gsm (2),

nb-iot (3),

nr-v1510 (4) } (SIZE (1..8)),

...

}

-- ASN1STOP

| *AccessTypes* field descriptions |
| --- |
| ***accessTypes***  This field specifies the cellular access type(s). This is represented by a bit string, with a one‑value at the bit position means the particular access type is addressed; a zero‑value means not addressed. |

#### *–* *ARFCN-ValueEUTRA*

The IEs *ARFCN-ValueEUTRA* and *ARFCN-ValueEUTRA-v9a0* are used to indicate the ARFCN of the E-UTRA carrier frequency, as defined in TS 36.331 [12].

-- ASN1START

ARFCN-ValueEUTRA ::= INTEGER (0..maxEARFCN)

ARFCN-ValueEUTRA-v9a0 ::= INTEGER (maxEARFCN-Plus1..maxEARFCN2)

ARFCN-ValueEUTRA-r14 ::= INTEGER (0..maxEARFCN2)

-- ASN1STOP

NOTE 1: For fields using the original value range, as defined by IE *ARFCN-ValueEUTRA* i.e. without suffix, value *maxEARFCN* indicates that the E-UTRA carrier frequency is indicated by means of an extension.

#### – *ARFCN-ValueNR*

The IE *ARFCN-ValueNR* is used to indicate the ARFCN applicable for a downlink, uplink or bi-directional (TDD) NR global frequency raster, as defined in TS 38.101-2 [34] and TS 38.101-1 [37].

-- ASN1START

ARFCN-ValueNR-r15 ::= INTEGER (0..3279165)

-- ASN1STOP

#### *– ARFCN-ValueUTRA*

The IE *ARFCN-ValueUTRA* is used to indicate the ARFCN of the UTRA carrier frequency, as defined in TS 25.331 [13].

-- ASN1START

ARFCN-ValueUTRA ::= INTEGER (0..16383)

-- ASN1STOP

#### – *CarrierFreq-NB*

The IE *CarrierFreq-NB* is used to provide the NB-IoT carrier frequency, as defined in TS 36.101 [21].

-- ASN1START

CarrierFreq-NB-r14 ::= SEQUENCE {

carrierFreq-r14 ARFCN-ValueEUTRA-r14,

carrierFreqOffset-r14 CarrierFreqOffsetNB-r14 OPTIONAL,

...

}

-- ASN1STOP

| *CarrierFreq-NB* field descriptions |
| --- |
| ***carrierFreq***  This field specifies the ARFCN applicable for the NB-IoT carrier frequency as defined in TS 36.101 [21, Table 5.7.3-1]. |
| ***carrierFreqOffset***  This field specifies the offset of the NB-IoT channel number to EARFCN as defined in TS 36.101 [21]. |

– *CarrierFreqOffsetNB*

The IE *CarrierFreqOffsetNB* is used to provide the offset of the NB-IoT channel number to EARFCN of a NB-IoT carrier.

-- ASN1START

CarrierFreqOffsetNB-r14 ::= ENUMERATED {

v-10, v-9, v-8, v-7, v-6, v-5, v-4, v-3, v-2, v-1, v-0dot5,

v0, v1, v2, v3, v4, v5, v6, v7, v8, v9

}

-- ASN1STOP

| *CarrierFreqOffsetNB field descriptions* |
| --- |
| ***CarrierFreqOffsetNB***  This field specifies the offset of the NB-IoT channel number to EARFCN as defined in TS 36.101 [21]. Value v-10 means -10, v-9 means -9, and so on. |

#### *– CellGlobalIdEUTRA-AndUTRA*

The IE *CellGlobalIdEUTRA-AndUTRA* specifies the global Cell Identifier for E‑UTRA or UTRA, the globally unique identity of a cell in E‑UTRA or UTRA.

-- ASN1START

CellGlobalIdEUTRA-AndUTRA ::= SEQUENCE {

plmn-Identity SEQUENCE {

mcc SEQUENCE (SIZE (3)) OF INTEGER (0..9),

mnc SEQUENCE (SIZE (2..3)) OF INTEGER (0..9)

},

cellIdentity CHOICE {

eutra BIT STRING (SIZE (28)),

utra BIT STRING (SIZE (32))

},

...

}

-- ASN1STOP

| ***CellGlobalIdEUTRA-AndUTRA* field descriptions** |
| --- |
| ***plmn-Identity***  This field identifies the PLMN of the cell as defined in TS 36.331 [12]. |
| ***cellIdentity***  This field defines the identity of the cell within the context of the PLMN as defined in TS 36.331 [12] and TS 25.331 [13]. The size of the bit string allows for the 32-bit extended UTRAN cell ID; in the case the cell ID is shorter, the first bits of the string are set to 0. |

#### *– CellGlobalIdGERAN*

The IE *CellGlobalIdGERAN* specifies the global Cell Identifier for GERAN, the globally unique identity of a cell in GERAN.

-- ASN1START

CellGlobalIdGERAN ::= SEQUENCE {

plmn-Identity SEQUENCE {

mcc SEQUENCE (SIZE (3)) OF INTEGER (0..9),

mnc SEQUENCE (SIZE (2..3)) OF INTEGER (0..9)

},

locationAreaCode BIT STRING (SIZE (16)),

cellIdentity BIT STRING (SIZE (16)),

...

}

-- ASN1STOP

| ***CellGlobalIdGERAN* field descriptions** |
| --- |
| ***plmn-Identity***  This field identifies the PLMN of the cell. |
| ***locationAreaCode***  This field is a fixed length code identifying the location area within a PLMN. |
| ***cellIdentity***  This field specifies the cell Identifier which is unique within the context of the GERAN location area. |

#### *– ECGI*

The IE *ECGI* specifies the Evolved Cell Global Identifier (ECGI), the globally unique identity of a cell in E-UTRA (TS 36.331 [12]).

NOTE 2: The IE *ECGI* is also used for NB-IoT access.

-- ASN1START

ECGI ::= SEQUENCE {

mcc SEQUENCE (SIZE (3)) OF INTEGER (0..9),

mnc SEQUENCE (SIZE (2..3)) OF INTEGER (0..9),

cellidentity BIT STRING (SIZE (28))

}

-- ASN1STOP

#### *– Ellipsoid-Point*

The IE *Ellipsoid-Point* is used to describe a geographic shape as defined in TS 23.032 [15].

-- ASN1START

Ellipsoid-Point ::= SEQUENCE {

latitudeSign ENUMERATED {north, south},

degreesLatitude INTEGER (0..8388607), -- 23 bit field

degreesLongitude INTEGER (-8388608..8388607) -- 24 bit field

}

-- ASN1STOP

#### *– Ellipsoid-PointWithUncertaintyCircle*

The IE *Ellipsoid-PointWithUncertaintyCircle* is used to describe a geographic shape as defined in TS 23.032 [15].

-- ASN1START

Ellipsoid-PointWithUncertaintyCircle ::= SEQUENCE {

latitudeSign ENUMERATED {north, south},

degreesLatitude INTEGER (0..8388607), -- 23 bit field

degreesLongitude INTEGER (-8388608..8388607), -- 24 bit field

uncertainty INTEGER (0..127)

}

-- ASN1STOP

#### *– EllipsoidPointWithUncertaintyEllipse*

The IE *EllipsoidPointWithUncertaintyEllipse* is used to describe a geographic shape as defined in TS 23.032 [15].

-- ASN1START

EllipsoidPointWithUncertaintyEllipse ::= SEQUENCE {

latitudeSign ENUMERATED {north, south},

degreesLatitude INTEGER (0..8388607), -- 23 bit field

degreesLongitude INTEGER (-8388608..8388607), -- 24 bit field

uncertaintySemiMajor INTEGER (0..127),

uncertaintySemiMinor INTEGER (0..127),

orientationMajorAxis INTEGER (0..179),

confidence INTEGER (0..100)

}

-- ASN1STOP

#### *– EllipsoidPointWithAltitude*

The IE *EllipsoidPointWithAltitude* is used to describe a geographic shape as defined in TS 23.032 [15].

-- ASN1START

EllipsoidPointWithAltitude ::= SEQUENCE {

latitudeSign ENUMERATED {north, south},

degreesLatitude INTEGER (0..8388607), -- 23 bit field

degreesLongitude INTEGER (-8388608..8388607), -- 24 bit field

altitudeDirection ENUMERATED {height, depth},

altitude INTEGER (0..32767) -- 15 bit field

}

-- ASN1STOP

#### *– EllipsoidPointWithAltitudeAndUncertaintyEllipsoid*

The IE *EllipsoidPointWithAltitudeAndUncertaintyEllipsoid* is used to describe a geographic shape as defined in TS 23.032 [15].

-- ASN1START

EllipsoidPointWithAltitudeAndUncertaintyEllipsoid ::= SEQUENCE {

latitudeSign ENUMERATED {north, south},

degreesLatitude INTEGER (0..8388607), -- 23 bit field

degreesLongitude INTEGER (-8388608..8388607), -- 24 bit field

altitudeDirection ENUMERATED {height, depth},

altitude INTEGER (0..32767), -- 15 bit field

uncertaintySemiMajor INTEGER (0..127),

uncertaintySemiMinor INTEGER (0..127),

orientationMajorAxis INTEGER (0..179),

uncertaintyAltitude INTEGER (0..127),

confidence INTEGER (0..100)

}

-- ASN1STOP

#### *– EllipsoidArc*

The IE *EllipsoidArc* is used to describe a geographic shape as defined in TS 23.032 [15].

-- ASN1START

EllipsoidArc ::= SEQUENCE {

latitudeSign ENUMERATED {north, south},

degreesLatitude INTEGER (0..8388607), -- 23 bit field

degreesLongitude INTEGER (-8388608..8388607), -- 24 bit field

innerRadius INTEGER (0..65535), -- 16 bit field,

uncertaintyRadius INTEGER (0..127),

offsetAngle INTEGER (0..179),

includedAngle INTEGER (0..179),

confidence INTEGER (0..100)

}

-- ASN1STOP

#### *– EPDU-Sequence*

The *EPDU-Sequence* contains IEs that are defined externally to LPP by other organizations.

-- ASN1START

EPDU-Sequence ::= SEQUENCE (SIZE (1..maxEPDU)) OF EPDU

maxEPDU INTEGER ::= 16

EPDU ::= SEQUENCE {

ePDU-Identifier EPDU-Identifier,

ePDU-Body EPDU-Body

}

EPDU-Identifier ::= SEQUENCE {

ePDU-ID EPDU-ID,

ePDU-Name EPDU-Name OPTIONAL,

...

}

EPDU-ID ::= INTEGER (1..256)

EPDU-Name ::= VisibleString (SIZE (1..32))

EPDU-Body ::= OCTET STRING

-- ASN1STOP

| ***EPDU-Sequence* field descriptions** |
| --- |
| ***EPDU-ID***  This field provides a unique integer ID for the externally defined positioning method. Its value is assigned to the external entity that defines the EPDU. See table External PDU Identifier Definition for a list of external PDU identifiers defined in this version of the specification. |
| ***EPDU-Name***  This field provides an optional character encoding which can be used to provide a quasi-unique name for an external PDU – e.g., by containing the name of the defining organization and/or the name of the associated public or proprietary standard for the EPDU. |
| ***EPDU-Body***  The content and encoding of this field are defined externally to LPP. |

External PDU Identifier Definition

|  |  |  |  |
| --- | --- | --- | --- |
| EPDU-ID | EPDU Defining entity | Method name | Reference |
| 1 | OMA LOC | OMA LPP extensions (LPPe) | OMA-TS-LPPe-V1\_0 [20] |

#### *– FreqBandIndicatorNR*

The IE *FreqBandIndicatorNR* specifies the NR band indicator (TS 38.331 [35]).

-- ASN1START

FreqBandIndicatorNR-r16 ::= INTEGER (1..1024)

-- ASN1STOP

#### – *HA-EllipsoidPointWithAltitudeAndScalableUncertaintyEllipsoid*

The IE *HA-EllipsoidPointWithAltitudeAndScalableUncertaintyEllipsoid* is used to describe a geographic shape as defined in TS 23.032 [15].

-- ASN1START

HA-EllipsoidPointWithAltitudeAndScalableUncertaintyEllipsoid-r16 ::= SEQUENCE {

degreesLatitude-r16 INTEGER(-2147483648..2147483647),

degreesLongitude-r16 INTEGER(-2147483648..2147483647),

altitude-r16 INTEGER(-64000..1280000),

uncertaintySemiMajor-r16 INTEGER (0..255),

uncertaintySemiMinor-r16 INTEGER (0..255),

orientationMajorAxis-r16 INTEGER (0..179),

horizontalConfidence-r16 INTEGER (0..100),

uncertaintyAltitude-r16 INTEGER (0..255),

verticalConfidence-r16 INTEGER (0..100),

ha-HorizontalExtendedRangeUsed-r16 BOOLEAN,

ha-VerticalExtendedRangeUsed-r16 BOOLEAN

}

-- ASN1STOP

#### – *HA-EllipsoidPointWithScalableUncertaintyEllipse*

The IE *HA-EllipsoidPointWithScalableUncertaintyEllipse* is used to describe a geographic shape as defined in TS 23.032 [15].

-- ASN1START

HA-EllipsoidPointWithScalableUncertaintyEllipse-r16 ::= SEQUENCE {

degreesLatitude-r16 INTEGER(-2147483648..2147483647),

degreesLongitude-r16 INTEGER(-2147483648..2147483647),

uncertaintySemiMajor-r16 INTEGER (0..255),

uncertaintySemiMinor-r16 INTEGER (0..255),

orientationMajorAxis-r16 INTEGER (0..179),

confidence-r16 INTEGER (0..100),

ha-ExtendedUncertaintyRangeUsed-r16 BOOLEAN

}

-- ASN1STOP

#### *– HighAccuracyEllipsoidPointWithUncertaintyEllipse*

The IE *HighAccuracyEllipsoidPointWithUncertaintyEllipse* is used to describe a geographic shape as defined in TS 23.032 [15].

-- ASN1START

HighAccuracyEllipsoidPointWithUncertaintyEllipse-r15 ::= SEQUENCE {

degreesLatitude-r15 INTEGER(-2147483648..2147483647),

degreesLongitude-r15 INTEGER(-2147483648..2147483647),

uncertaintySemiMajor-r15 INTEGER (0..255),

uncertaintySemiMinor-r15 INTEGER (0..255),

orientationMajorAxis-r15 INTEGER (0..179),

confidence-r15 INTEGER (0..100)

}

-- ASN1STOP

#### *– HighAccuracyEllipsoidPointWithAltitudeAndUncertaintyEllipsoid*

The IE *HighAccuracyEllipsoidPointWithAltitudeAndUncertaintyEllipsoid* is used to describe a geographic shape as defined in TS 23.032 [15].

-- ASN1START

HighAccuracyEllipsoidPointWithAltitudeAndUncertaintyEllipsoid-r15 ::= SEQUENCE {

degreesLatitude-r15 INTEGER(-2147483648..2147483647),

degreesLongitude-r15 INTEGER(-2147483648..2147483647),

altitude-r15 INTEGER(-64000..1280000),

uncertaintySemiMajor-r15 INTEGER (0..255),

uncertaintySemiMinor-r15 INTEGER (0..255),

orientationMajorAxis-r15 INTEGER (0..179),

horizontalConfidence-r15 INTEGER (0..100),

uncertaintyAltitude-r15 INTEGER (0..255),

verticalConfidence-r15 INTEGER (0..100)

}

-- ASN1STOP

#### *– HorizontalVelocity*

The IE *HorizontalVelocity* is used to describe a velocity shape as defined in TS 23.032 [15].

-- ASN1START

HorizontalVelocity ::= SEQUENCE {

bearing INTEGER(0..359),

horizontalSpeed INTEGER(0..2047)

}

-- ASN1STOP

#### *– HorizontalWithVerticalVelocity*

The IE *HorizontalWithVerticalVelocity* is used to describe a velocity shape as defined in TS 23.032 [15].

-- ASN1START

HorizontalWithVerticalVelocity ::= SEQUENCE {

bearing INTEGER(0..359),

horizontalSpeed INTEGER(0..2047),

verticalDirection ENUMERATED{upward, downward},

verticalSpeed INTEGER(0..255)

}

-- ASN1STOP

#### *– HorizontalVelocityWithUncertainty*

The IE *HorizontalVelocityWithUncertainty* is used to describe a velocity shape as defined in TS 23.032 [15].

-- ASN1START

HorizontalVelocityWithUncertainty ::= SEQUENCE {

bearing INTEGER(0..359),

horizontalSpeed INTEGER(0..2047),

uncertaintySpeed INTEGER(0..255)

}

-- ASN1STOP

#### *– HorizontalWithVerticalVelocityAndUncertainty*

The IE *HorizontalWithVerticalVelocityAndUncertainty* is used to describe a velocity shape as defined in TS 23.032 [15].

-- ASN1START

HorizontalWithVerticalVelocityAndUncertainty ::= SEQUENCE {

bearing INTEGER(0..359),

horizontalSpeed INTEGER(0..2047),

verticalDirection ENUMERATED{upward, downward},

verticalSpeed INTEGER(0..255),

horizontalUncertaintySpeed INTEGER(0..255),

verticalUncertaintySpeed INTEGER(0..255)

}

-- ASN1STOP

#### *– Local2dPointWithUncertaintyEllipse*

The IE *Local2dPointWithUncertaintyEllipse* is used to describe a geographic shape as defined in TS 23.032 [15].

-- ASN1START

Local2dPointWithUncertaintyEllipse-r18 ::= SEQUENCE {

localOrigin-r18 ReferencePoint-r16,

cartesianCoordinatesUnits-r18 ENUMERATED { mm, cm, dm, m, ...},

x-value-r18 X-Value-r18,

y-value-r18 Y-Value-r18,

uncertaintySemiMajor-r18 INTEGER (0..127),

uncertaintySemiMinor-r18 INTEGER (0..127),

orientationMajorAxis-r18 INTEGER (0..179),

confidence-r18 INTEGER (0..100)

}

-- ASN1STOP

| *Local2dPointWithUncertaintyEllipse* field descriptions |
| --- |
| ***localOrigin***  This field identifies the reference point of the local Cartesian coordinate system. |
| ***cartesianCoordinatesUnits***  This field provides the unit and scale factor for the *x-value* and *y-value* fields. Enumerated values mm, cm, dm, and m, correspond to 10-3 metre, 10-2 metre, 10-1 metre and 1 metres, respectively. |
| ***x-value***  This field provides the x-value of the location in the Cartesian coordinate system. Positive value represents easting from reference point (origin) [15], unless *horizAxesOrientation* is provided in the *LocalOrigin*, in which case the local coordinate system is rotated clockwise horizontally by *horizAxesOrientation*). See IE *RelativeCartesianLocation*. |
| ***y-value***  This field provides the y-value of the location in the Cartesian coordinate system. Positive value represents northing from reference point (origin) [15], unless *horizAxesOrientation* is provided in the *LocalOrigin*, in which case the local coordinate system is rotated clockwise horizontally by *horizAxesOrientation*). See IE *RelativeCartesianLocation*. |
| ***uncertaintySemiMajor***  This field indicates the semi-major axis of the uncertainty ellipse [15]. |
| ***uncertaintySemiMinor***  This field indicates the semi-minor axis of the uncertainty ellipse [15]. |
| ***orientationMajorAxis***  This field indicates the orientation angle of the major axis [15] in relation to the local Cartesian coordinate system defined by the *localOrigin*, where the *orientationMajoAxis* angle is clockwise from the y-axis. |
| ***confidence***  This field indicates the confidence value [15]. |

#### *– Local3dPointWithUncertaintyEllipsoid*

The IE *Local3dPointWithUncertaintyEllipsoid* is used to describe a geographic shape as defined in TS 23.032 [15].

-- ASN1START

Local3dPointWithUncertaintyEllipsoid-r18 ::= SEQUENCE {

localOrigin-r18 ReferencePoint-r16,

cartesianCoordinatesUnits-r18 ENUMERATED { mm, cm, dm, m, ...},

x-value-r18 X-Value-r18,

y-value-r18 Y-Value-r18,

z-value-r18 Z-Value-r18,

uncertaintySemiMajor-r18 INTEGER (0..127),

uncertaintySemiMinor-r18 INTEGER (0..127),

orientationMajorAxis-r18 INTEGER (0..179),

uncertaintyAltitude-r18 INTEGER (0..127),

confidence-r18 INTEGER (0..100),

vConfidence-r18 INTEGER (0..100) OPTIONAL -- Need ON

}

-- ASN1STOP

| *Local3dPointWithUncertaintyEllipsoid* field descriptions |
| --- |
| ***localOrigin***  This field identifies the reference point of the local Cartesian coordinate system. |
| ***cartesianCoordinatesUnits***  This field provides the unit and scale factor for the *x-value*, *y-value* and *z-value* fields. Enumerated values mm, cm, dm, and m, correspond to 10-3 metre, 10-2 metre, 10-1 metre and 1 metres, respectively. |
| ***x-value***  This field provides the x-value of the location in the Cartesian coordinate system. Positive value represents easting from reference point (origin) [15], unless *horizAxesOrientation* is provided in the *LocalOrigin*, in which case the local coordinate system is rotated clockwise horizontally by *horizAxesOrientation*). See IE *RelativeCartesianLocation*. |
| ***y-value***  This field provides the y-value of the location in the Cartesian coordinate system. Positive value represents northing from reference point (origin) [15], unless *horizAxesOrientation* is provided in the *LocalOrigin*, in which case the local coordinate system is rotated clockwise horizontally by *horizAxesOrientation*). See IE *RelativeCartesianLocation*. |
| ***z-value***  This field provides the z-value of the location in the Cartesian coordinate system. Positive value represents height above reference point (origin) [15]. See IE *RelativeCartesianLocation*. |
| ***uncertaintySemiMajor***  This field indicates the semi-major axis of the uncertainty ellipsoid [15]. |
| ***uncertaintySemiMinor***  This field indicates the semi-minor axis of the uncertainty ellipsoid [15]. |
| ***orientationMajorAxis***  This field indicates the orientation angle of the major axis [15], in relation to the local Cartesian coordinate system defined by the *localOrigin*, where the *orientationMajorAxis* angle is clockwise from the y-axis. |
| ***uncertaintyAltitude***  This field indicates the vertical axis of the uncertainty ellipsoid [15]. |
| ***confidence***  This field indicates the confidence value [15]. If the *vConfidence* field is present, this field shall indicate the value of horizontal confidence. |
| ***vConfidence***  This field indicates the vertical confidence value [15]. |

#### *– LocationCoordinateTypes*

The IE *LocationCoordinateTypes* defines a list of possible geographic shapes as defined in TS 23.032 [15].

-- ASN1START

LocationCoordinateTypes ::= SEQUENCE {

ellipsoidPoint BOOLEAN,

ellipsoidPointWithUncertaintyCircle BOOLEAN,

ellipsoidPointWithUncertaintyEllipse BOOLEAN,

polygon BOOLEAN,

ellipsoidPointWithAltitude BOOLEAN,

ellipsoidPointWithAltitudeAndUncertaintyEllipsoid BOOLEAN,

ellipsoidArc BOOLEAN,

...,

[[

highAccuracyEllipsoidPointWithUncertaintyEllipse-r15

BOOLEAN OPTIONAL, -- Need ON

highAccuracyEllipsoidPointWithAltitudeAndUncertaintyEllipsoid-r15

BOOLEAN OPTIONAL -- Need ON

]],

[[

ha-EllipsoidPointWithScalableUncertaintyEllipse-r16

BOOLEAN OPTIONAL, -- Need ON

ha-EllipsoidPointWithAltitudeAndScalableUncertaintyEllipsoid-r16

BOOLEAN OPTIONAL -- Need ON

]],

[[

local2dPointWithUncertaintyEllipse-r18 BOOLEAN OPTIONAL, -- Need ON

local3dPointWithUncertaintyEllipsoid-r18 BOOLEAN OPTIONAL -- Need ON

]]

}

-- ASN1STOP

NOTE 3: In this version of the specification, the GAD shapes *local2dPointWithUncertaintyEllipse* and *local3dPointWithUncertaintyEllipsoid* are supported for DL-TDOA and DL-AoD only.

#### *– NCGI*

The IE *NCGI* specifies the NR Cell Global Identifier (NCGI) which is used to identify NR cells globally (TS 38.331 [35]).

-- ASN1START

NCGI-r15 ::= SEQUENCE {

mcc-r15 SEQUENCE (SIZE (3)) OF INTEGER (0..9),

mnc-r15 SEQUENCE (SIZE (2..3)) OF INTEGER (0..9),

nr-cellidentity-r15 BIT STRING (SIZE (36))

}

-- ASN1STOP

#### *– NR-PhysCellId*

The IE *NR-PhysCellId* specifies the NR physical cell identifier (TS 38.331 [35]).

-- ASN1START

NR-PhysCellID-r16 ::= INTEGER (0..1007)

-- ASN1STOP

#### *– PeriodicAssistanceDataControlParameters*

The IE *PeriodicAssistanceDataControlParameters* is used in a periodic assistance data delivery procedure as described in clauses 5.2.1a and 5.2.2a.

-- ASN1START

PeriodicAssistanceDataControlParameters-r15 ::= SEQUENCE {

periodicSessionID-r15 PeriodicSessionID-r15,

...,

[[

updateCapabilities-r15 UpdateCapabilities-r15 OPTIONAL -- Need ON

]]

}

PeriodicSessionID-r15 ::= SEQUENCE {

periodicSessionInitiator-r15 ENUMERATED { locationServer, targetDevice, ... },

periodicSessionNumber-r15 INTEGER (0..255),

...

}

UpdateCapabilities-r15 ::= BIT STRING {primaryCellID-r15 (0)} (SIZE(1..8))

-- ASN1STOP

| *PeriodicAssistanceDataControlParameters* field descriptions |
| --- |
| ***periodicSessionID***  This field identifies a particular periodic assistance data delivery session and the initiator of the session. |
| ***updateCapabilities***  This field identifies the capabilities of the sending entity to support an update of periodic assistance data. A bit value set to one indicates a capability is supported and a bit value set to zero indicates a capability is not supported. |

#### *– PeriodicReportingIntervalMsSupport*

The IE *PeriodicReportingIntervalMsSupport* is used by the target device to indicate if millisecond reporting intervals are supported by providing the minimum millisecond reporting interval for periodic location information reporting.

-- ASN1START

PeriodicReportingIntervalMsSupport-r18 ::= SEQUENCE {

minPeriodicReportingIntervalMs-r18 ENUMERATED {ms1, ms10, ms100,...},

...

}

-- ASN1STOP

| *PeriodicReportingIntervalMsSupport* field descriptions |
| --- |
| ***minPeriodicReportingIntervalMs***  This field indicates the minimum sub-second periodic reporting interval supported by the target device, where ms1, ms10, ms100 corresponds to 1, 10, and 100 milliseconds respectively. |

#### *– PeriodicReportingIntervalMsSupportPerMode*

The IE *PeriodicReportingIntervalMsSupportPerMode* is used by the target device to indicate if millisecond reporting intervals are supported by providing the minimum millisecond reporting interval for periodic location information reporting for each positioning mode indicated by *PositioningModes*.

-- ASN1START

PeriodicReportingIntervalMsSupportPerMode-r18 ::= SEQUENCE {

minPeriodicReportingIntervalMs1-Supported-r18 PositioningModes OPTIONAL,

minPeriodicReportingIntervalMs10-Supported-r18 PositioningModes OPTIONAL,

minPeriodicReportingIntervalMs100-Supported-r18 PositioningModes OPTIONAL,

...

}

-- ASN1STOP

| *PeriodicReportingIntervalMsSupportPerMode* field descriptions |
| --- |
| ***minPeriodicReportingIntervalMs1-Supported***  This field indicates the positioning modes of the target device supporting a minimum of 1 millisecond periodic reporting interval. |
| ***minPeriodicReportingIntervalMs10-Supported***  This field indicates the positioning modes of the target device supporting a minimum of 10 millisecond periodic reporting interval. |
| ***minPeriodicReportingIntervalMs100-Supported***  This field indicates the positioning modes of the target device supporting a minimum of 100 millisecond periodic reporting interval. |

#### *– Polygon*

The IE *Polygon* is used to describe a geographic shape as defined in TS 23.032 [15].

-- ASN1START

Polygon ::= SEQUENCE (SIZE (3..15)) OF PolygonPoints

PolygonPoints ::= SEQUENCE {

latitudeSign ENUMERATED {north, south},

degreesLatitude INTEGER (0..8388607), -- 23 bit field

degreesLongitude INTEGER (-8388608..8388607) -- 24 bit field

}

-- ASN1STOP

#### *– PositioningModes*

The IE *PositioningModes* is used to indicate several positioning modes using a bit map.

-- ASN1START

PositioningModes ::= SEQUENCE {

posModes BIT STRING { standalone (0),

ue-based (1),

ue-assisted (2)

} (SIZE (1..8)),

...

}

-- ASN1STOP

| *PositioningModes* field descriptions |
| --- |
| ***posModes***  This field specifies the positioning mode(s). This is represented by a bit string, with a one‑value at the bit position means the particular positioning mode is addressed; a zero‑value means not addressed. |

#### *– ScheduledLocationTimeSupport*

The IE *ScheduledLocationTimeSupport* is used by the target device to indicate the time bases supported for scheduled location requests.

-- ASN1START

ScheduledLocationTimeSupport-r17 ::= SEQUENCE {

utcTime-r17 ENUMERATED { supported } OPTIONAL,

gnssTime-r17 GNSS-ID-Bitmap OPTIONAL,

e-utraTime-r17 ENUMERATED { supported } OPTIONAL,

nrTime-r17 ENUMERATED { supported } OPTIONAL,

relativeTime-r17 ENUMERATED { supported } OPTIONAL,

...

}

-- ASN1STOP

#### *– ScheduledLocationTimeSupportPerMode*

The IE *ScheduledLocationTimeSupportPerMode* is used by the target device to indicate the time bases supported for scheduled location requests for each positioning mode indicated by *PositioningModes*.

-- ASN1START

ScheduledLocationTimeSupportPerMode-r17 ::= SEQUENCE {

utcTime-r17 PositioningModes OPTIONAL,

gnssTime-r17 SEQUENCE {

posModes-r17 PositioningModes,

gnss-TimeIDs-r17 GNSS-ID-Bitmap

} OPTIONAL,

e-utraTime-r17 PositioningModes OPTIONAL,

nrTime-r17 PositioningModes OPTIONAL,

relativeTime-r17 PositioningModes OPTIONAL,

...

}

-- ASN1STOP

#### – *SegmentationInfo*

The IE *SegmentationInfo* is used by a sender to indicate that LPP message segmentation is used, as specified in clause 4.3.5.

-- ASN1START

SegmentationInfo-r14 ::= ENUMERATED { noMoreMessages, moreMessagesOnTheWay }

-- ASN1STOP

| *SegmentationInfo* field descriptions |
| --- |
| ***SegmentationInfo***  *noMoreMessages* indicates that this is the only or last LPP message segment used to deliver the entire message body.  *moreMessagesOnTheWay* indicates that this is one of multiple LPP messagesegments used to deliver the entire message body. |

#### *– VelocityTypes*

The IE *VelocityTypes* defines a list of possible velocity shapes as defined in TS 23.032 [15].

-- ASN1START

VelocityTypes ::= SEQUENCE {

horizontalVelocity BOOLEAN,

horizontalWithVerticalVelocity BOOLEAN,

horizontalVelocityWithUncertainty BOOLEAN,

horizontalWithVerticalVelocityAndUncertainty BOOLEAN,

...

}

-- ASN1STOP

### 6.4.2 Common Positioning

#### – *CommonIEsRequestCapabilities*

The *CommonIEsRequestCapabilities* carries common IEs for a Request Capabilities LPP message Type.

-- ASN1START

CommonIEsRequestCapabilities ::= SEQUENCE {

...,

[[

lpp-message-segmentation-req-r14 BIT STRING { serverToTarget (0),

targetToServer (1) } OPTIONAL -- Need ON

]],

[[

remoteUE-IndicationReq-r18 ENUMERATED { true } OPTIONAL -- Cond NR

]]

}

-- ASN1STOP

| Conditional presence | Explanation |
| --- | --- |
| *NR* | This field is optionally present, need ON, for NR access. Otherwise it is not present. |

| *CommonIEsRequestCapabilities* field descriptions |
| --- |
| ***lpp-message-segmentation-req***  This field, if present, indicates that the target device is requested to provide its LPP message segmentation capabilities.  If bit 0 is set to value 1, it indicates that the server is able to send segmented LPP messages to the target device; if bit 0 is set to value 0 it indicates that the server is not able to send segmented LPP messages to the target device.  If bit 1 is set to value 1, it indicates that the server is able to receive segmented LPP messages from the target device; if bit 1 is set to value 0 it indicates that the server is not able to receive segmented LPP messages from the target device. |
| ***remoteUE-IndicationReq***  This field, if present, indicates that the target device is requested to indicate if it operates as a L2 U2N Remote UE. |

#### – *CommonIEsProvideCapabilities*

The *CommonIEsProvideCapabilities* carries common IEs for a Provide Capabilities LPP message Type.

-- ASN1START

CommonIEsProvideCapabilities ::= SEQUENCE {

...,

[[

segmentationInfo-r14 SegmentationInfo-r14 OPTIONAL, -- Cond Segmentation

lpp-message-segmentation-r14 BIT STRING { serverToTarget (0),

targetToServer (1) } OPTIONAL

]],

[[

remoteUE-Indication-r18 BOOLEAN OPTIONAL, -- Cond NR

locationEstimateAndMeasurementReporting-r18 ENUMERATED { supported } OPTIONAL

]]

}

-- ASN1STOP

| Conditional presence | Explanation |
| --- | --- |
| *Segmentation* | This field is optionally present, need OP, if *lpp-message-segmentation-req* has been received from the location server with bit 1 (*targetToServer*) set to value 1. The field shall be omitted if *lpp‑message‑segmentation-req* has not been received in this location session, or has been received with bit 1 (*targetToServer*) set to value 0. |
| *NR* | This field is optionally present for NR access if *remoteUE-IndicationReq* has been received from the location server in this location session. Otherwise it is not present. |

| *CommonIEsProvideCapabilities* field descriptions |
| --- |
| ***segmentationInfo***  This field indicates whether this *ProvideCapabilities* message is one of many segments, as specified in clause 4.3.5. |
| ***lpp-message-segmentation***  This field, if present, indicates the target device's LPP message segmentation capabilities.  If bit 0 is set to value 1, it indicates that the target device supports receiving segmented LPP messages; if bit 0 is set to value 0 it indicates that the target device does not support receiving segmented LPP messages.  If bit 1 is set to value 1, it indicates that the target device supports sending segmented LPP messages; if bit 1 is set to value 0 it indicates that the target device does not support sending segmented LPP messages. |
| ***remoteUE-Indication***  This field indicates whether the target device in NR access is configured as a L2 U2N Remote UE. The target device in NR access may transmit a *ProvideCapabilities* message with an appropriate value of this field when it starts or stops operation as a U2N Remote UE. |
| ***locationEstimateAndMeasurementReporting***  This field, if present, indicates that the PRU supports *locationEstimateAndMeasurementsRequired* in *LocationInformationType*.  NOTE: In this version of the specification, this capability is only applicable to PRUs. |

#### – *CommonIEsRequestAssistanceData*

The *CommonIEsRequestAssistanceData* carries common IEs for a Request Assistance Data LPP message Type.

-- ASN1START

CommonIEsRequestAssistanceData ::= SEQUENCE {

primaryCellID ECGI OPTIONAL, -- Cond EUTRA

...,

[[

segmentationInfo-r14 SegmentationInfo-r14 OPTIONAL -- Cond Segmentation

]],

[[

periodicAssistanceDataReq-r15

PeriodicAssistanceDataControlParameters-r15

OPTIONAL, -- Cond PerADreq

primaryCellID-r15 NCGI-r15 OPTIONAL -- Cond NR

]]

}

-- ASN1STOP

| Conditional presence | Explanation |
| --- | --- |
| *EUTRA* | The field is mandatory present for E-UTRA or NB-IoT access. The field shall be omitted for non-EUTRA and non-NB-IoT user plane support. |
| *Segmentation* | This field is optionally present, need OP, if *lpp-message-segmentation-req* has been received from the location server with bit 1 (*targetToServer*) set to value 1. The field shall be omitted if *lpp‑message‑segmentation-req* has not been received in this location session, or has been received with bit 1 (*targetToServer*) set to value 0. |
| *PerADreq* | The field is mandatory present if the target device requests periodic assistance data delivery. Otherwise it is not present. |
| *NR* | The field is mandatory present for NR access. The field shall be omitted for non-NR user plane support. |

| *CommonIEsRequestAssistanceData* field descriptions |
| --- |
| ***primaryCellID***  This parameter identifies the current primary cell for the target device. |
| ***segmentationInfo***  This field indicates whether this *RequestAssistanceData* message is one of many segments, as specified in clause 4.3.5. |
| ***periodicAssistanceDataReq***  This field indicates a request for periodic assistance data delivery, as specified in clause 5.2.1a. |

#### – *CommonIEsProvideAssistanceData*

The *CommonIEsProvideAssistanceData* carries common IEs for a Provide Assistance Data LPP message Type.

-- ASN1START

CommonIEsProvideAssistanceData ::= SEQUENCE {

...,

[[

segmentationInfo-r14 SegmentationInfo-r14 OPTIONAL -- Need ON

]],

[[

periodicAssistanceData-r15 PeriodicAssistanceDataControlParameters-r15

OPTIONAL -- Cond PerAD

]]

}

-- ASN1STOP

| Conditional presence | Explanation |
| --- | --- |
| *PerAD* | The field is mandatory present in a periodic assistance data delivery session. Otherwise it is not present. |

| *CommonIEsProvideAssistanceData* field descriptions |
| --- |
| ***segmentationInfo***  This field indicates whether this *ProvideAssistanceData* message is one of many segments, as specified in clause 4.3.5. |
| ***periodicAssistanceData***  This field indicates a periodic assistance data delivery, as specified in clauses 5.2.1a and 5.2.2a. |

#### – *CommonIEsRequestLocationInformation*

The *CommonIEsRequestLocationInformation* carries common IEs for a Request Location Information LPP message Type.

-- ASN1START

CommonIEsRequestLocationInformation ::= SEQUENCE {

locationInformationType LocationInformationType,

triggeredReporting TriggeredReportingCriteria OPTIONAL, -- Cond ECID

periodicalReporting PeriodicalReportingCriteria OPTIONAL, -- Need ON

additionalInformation AdditionalInformation OPTIONAL, -- Need ON

qos QoS OPTIONAL, -- Need ON

environment Environment OPTIONAL, -- Need ON

locationCoordinateTypes LocationCoordinateTypes OPTIONAL, -- Need ON

velocityTypes VelocityTypes OPTIONAL, -- Need ON

...,

[[

messageSizeLimitNB-r14 MessageSizeLimitNB-r14 OPTIONAL -- Need ON

]],

[[

segmentationInfo-r14 SegmentationInfo-r14 OPTIONAL -- Need ON

]],

[[

scheduledLocationTime-r17

ScheduledLocationTime-r17 OPTIONAL, -- Need ON

targetIntegrityRisk-r17

TargetIntegrityRisk-r17 OPTIONAL -- Need ON

]],

[[

periodicalReportingExt-r18

PeriodicalReportingCriteriaExt-r18

OPTIONAL -- Need ON

]]

}

LocationInformationType ::= ENUMERATED {

locationEstimateRequired,

locationMeasurementsRequired,

locationEstimatePreferred,

locationMeasurementsPreferred,

...,

locationEstimateAndMeasurementsRequired-r18

}

PeriodicalReportingCriteria ::= SEQUENCE {

reportingAmount ENUMERATED {

ra1, ra2, ra4, ra8, ra16, ra32,

ra64, ra-Infinity

} DEFAULT ra-Infinity,

reportingInterval ENUMERATED {

noPeriodicalReporting, ri0-25,

ri0-5, ri1, ri2, ri4, ri8, ri16, ri32, ri64

}

}

PeriodicalReportingCriteriaExt-r18 ::= SEQUENCE {

reportingAmount-r18 ENUMERATED {

ra2, ra4, ra8, ra16, ra32,

ra64, ra-Infinity

} DEFAULT ra-Infinity,

reportingIntervalMs-r18 INTEGER (1..999),

...

}

TriggeredReportingCriteria ::= SEQUENCE {

cellChange BOOLEAN,

reportingDuration ReportingDuration,

...

}

ReportingDuration ::= INTEGER (0..255)

AdditionalInformation ::= ENUMERATED {

onlyReturnInformationRequested,

mayReturnAdditionalInformation,

...

}

QoS ::= SEQUENCE {

horizontalAccuracy HorizontalAccuracy OPTIONAL, -- Need ON

verticalCoordinateRequest BOOLEAN,

verticalAccuracy VerticalAccuracy OPTIONAL, -- Need ON

responseTime ResponseTime OPTIONAL, -- Need ON

velocityRequest BOOLEAN,

...,

[[ responseTimeNB-r14 ResponseTimeNB-r14 OPTIONAL -- Need ON

]],

[[ horizontalAccuracyExt-r15 HorizontalAccuracyExt-r15 OPTIONAL, -- Need ON

verticalAccuracyExt-r15 VerticalAccuracyExt-r15 OPTIONAL -- Need ON

]]

}

HorizontalAccuracy ::= SEQUENCE {

accuracy INTEGER(0..127),

confidence INTEGER(0..100),

...

}

VerticalAccuracy ::= SEQUENCE {

accuracy INTEGER(0..127),

confidence INTEGER(0..100),

...

}

HorizontalAccuracyExt-r15 ::= SEQUENCE {

accuracyExt-r15 INTEGER(0..255),

confidence-r15 INTEGER(0..100),

...

}

VerticalAccuracyExt-r15 ::= SEQUENCE {

accuracyExt-r15 INTEGER(0..255),

confidence-r15 INTEGER(0..100),

...

}

ResponseTime ::= SEQUENCE {

time INTEGER (1..128),

...,

[[ responseTimeEarlyFix-r12 INTEGER (1..128) OPTIONAL -- Need ON

]],

[[ unit-r15 ENUMERATED { ten-seconds, ... , ten-milli-seconds-v1700 }

OPTIONAL -- Need ON

]]

}

ResponseTimeNB-r14 ::= SEQUENCE {

timeNB-r14 INTEGER (1..512),

responseTimeEarlyFixNB-r14 INTEGER (1..512) OPTIONAL, -- Need ON

...,

[[ unitNB-r15 ENUMERATED { ten-seconds, ... } OPTIONAL -- Need ON

]]

}

Environment ::= ENUMERATED {

badArea,

notBadArea,

mixedArea,

...

}

MessageSizeLimitNB-r14 ::= SEQUENCE {

measurementLimit-r14 INTEGER (1..512) OPTIONAL, -- Need ON

...

}

ScheduledLocationTime-r17 ::= SEQUENCE {

utcTime-r17 UTCTime OPTIONAL, -- Need ON

gnssTime-r17 SEQUENCE {

gnss-TOD-msec-r17 INTEGER (0..3599999),

gnss-TimeID-r17 GNSS-ID

} OPTIONAL, -- Need ON

networkTime-r17 CHOICE {

e-utraTime-r17 SEQUENCE {

lte-PhysCellId-r17 INTEGER (0..503),

lte-ArfcnEUTRA-r17 ARFCN-ValueEUTRA,

lte-CellGlobalId-r17 CellGlobalIdEUTRA-AndUTRA

OPTIONAL, -- Need ON

lte-SystemFrameNumber-r17 INTEGER (0..1023)

},

nrTime-r17 SEQUENCE {

nr-PhysCellID-r17 NR-PhysCellID-r16,

nr-ARFCN-r17 ARFCN-ValueNR-r15,

nr-CellGlobalID-r17 NCGI-r15 OPTIONAL, -- Need ON

nr-SFN-r17 INTEGER (0..1023),

nr-Slot-r17 CHOICE {

scs15-r17 INTEGER (0..9),

scs30-r17 INTEGER (0..19),

scs60-r17 INTEGER (0..39),

scs120-r17 INTEGER (0..79)

} OPTIONAL -- Need ON

},

...

} OPTIONAL, -- Need ON

relativeTime-r17 INTEGER (1..1024) OPTIONAL -- Need ON

}

TargetIntegrityRisk-r17 ::= INTEGER (10..90)

-- ASN1STOP

| Conditional presence | Explanation |
| --- | --- |
| *ECID* | The field is optionally present, need ON, if E-CID or NR E-CID is requested. Otherwise it is not present. |

| *CommonIEsRequestLocationInformation* field descriptions |
| --- |
| ***locationInformationType***  This IE indicates whether the server requires a location estimate or measurements. For '*locationEstimateRequired*', the target device shall return a location estimate if possible, or indicate a location error if not possible. For '*locationMeasurementsRequired*', the target device shall return measurements if possible, or indicate a location error if not possible. For '*locationEstimatePreferred*', the target device shall return a location estimate if possible, but may also or instead return measurements for any requested position methods for which a location estimate is not possible. For '*locationMeasurementsPreferred*', the target device shall return location measurements if possible, but may also or instead return a location estimate for any requested position methods for which return of location measurements is not possible. For '*locationEstimateAndMeasurementsRequired*', the PRU shall return both location estimate and measurements if possible, or indicate a measurements error if not possible.  NOTE: '*locationEstimateAndMeasurementsRequired*' only applies to PRUs. If the PRU is requested to return both location estimate and measurements, the location estimate is determined independently of the reported measurements, and the measurements shall be valid at the reported location. |
| ***triggeredReporting***  This IE indicates that triggered reporting is requested and comprises the following subfields:  - ***cellChange***: If this field is set to TRUE, the target device provides requested location information each time the primary cell has changed.  - ***reportingDuration***: Maximum duration of triggered reporting in seconds. A value of zero is interpreted to mean an unlimited (i.e. "infinite") duration. The target device should continue triggered reporting for the *reportingDuration* or until an LPP *Abort* or *LPP Error* message is received.  The *triggeredReporting* field should not be included by the location server and shall be ignored by the target device if the *periodicalReporting* IE or *responseTime* IE or *responseTimeNB* IE is included in *CommonIEsRequestLocationInformation.* |
| ***periodicalReporting***  This IE indicates that periodic reporting is requested and comprises the following subfields:  - ***reportingAmount*** indicates the number of periodic location information reports requested. Enumerated values correspond to 1, 2, 4, 8, 16, 32, 64, or infinite/indefinite number of reports. If the *reportingAmount* is '*infinite/indefinite'*, the target device shou-ld continue periodic reporting until an LPP *Abort* message is received. The value '*ra1*' shall not be used by a sender.  - ***reportingInterval*** indicates the interval between location information reports and the response time requirement for the first location information report. Enumerated values ri0-25, ri0-5, ri1, ri2, ri4, ri8, ri16, ri32, ri64 correspond to reporting intervals of 1, 2, 4, 8, 10, 16, 20, 32, and 64 seconds, respectively. Measurement reports containing no measurements or no location estimate are required when a *reportingInterval* expires before a target device is able to obtain new measurements or obtain a new location estimate. The value '*noPeriodicalReporting*' shall not be used by a sender. |
| ***additionalInformation***  This IE indicates whether a target device is allowed to return additional information to that requested. If this IE indicates '*onlyReturnInformationRequested'* then the target device shall not return any additional information to that requested by the server. If this IE indicates '*mayReturnAdditionalInformation'* then the target device may return additional information to that requested by the server. If a location estimate is returned, any additional information is restricted to that associated with a location estimate (e.g. might include velocity if velocity was not requested but cannot include measurements). If measurements are returned, any additional information is restricted to additional measurements (e.g. might include E-CID measurements if A-GNSS measurements were requested but not E-CID measurements). |
| ***qos***  This IE indicates the quality of service and comprises a number of sub-fields. In the case of measurements, some of the sub-fields apply to the location estimate that could be obtained by the server from the measurements provided by the target device assuming that the measurements are the only sources of error. Fields are as follows:  - ***horizontalAccuracy*** indicates the maximum horizontal error in the location estimate at an indicated confidence level. The '*accuracy*' corresponds to the encoded uncertainty as defined in TS 23.032 [15] and '*confidence*' corresponds to confidence as defined in TS 23.032 [15].  - ***verticalCoordinateRequest*** indicates whether a vertical coordinate is required (TRUE) or not (FALSE)  - ***verticalAccuracy*** indicates the maximum vertical error in the location estimate at an indicated confidence level and is only applicable when a vertical coordinate is requested. The '*accuracy*' corresponds to the encoded uncertainty altitude as defined in TS 23.032 [15] and '*confidence*' corresponds to confidence as defined in TS 23.032 [15].  - ***responseTime***  - ***time*** indicates the maximum response time as measured between receipt of the *RequestLocationInformation* and transmission of a *ProvideLocationInformation*. If the *unit* field is absent, this is given as an integer number of seconds between 1 and 128. If the *unit* field is present with enumerated value '*ten-seconds*', the maximum response time is given in units of 10-seconds, between 10 and 1280 seconds. If the *unit* field is present with enumerated value '*ten-milli-seconds*', the maximum response time is given in units of 10-milli-seconds, between 0.01 and 1.28 seconds. If the *periodicalReporting* IE is included in *CommonIEsRequestLocationInformation*, this field should not be included by the location server and shall be ignored by the target device (if included).  - ***responseTimeEarlyFix*** indicates the maximum response time as measured between receipt of the *RequestLocationInformation* and transmission of a *ProvideLocationInformation* containing early location measurements or an early location estimate. If the *unit* field is absent, this is given as an integer number of seconds between 1 and 128. If the *unit* field is present with enumerated value '*ten-seconds*', the maximum response time is given in units of 10-seconds, between 10 and 1280 seconds. If the *unit* field is present with enumerated value '*ten-milli-seconds*', the maximum response time is given in units of 10-milli-seconds, between 0.01 and 1.28 seconds. When this IE is included, a target should send a *ProvideLocationInformation* (or more than one *ProvideLocationInformation* if location information will not fit into a single message) containing early location information according to the *responseTimeEarlyFix* IE and a subsequent *ProvideLocationInformation* (or more than one *ProvideLocationInformation* if location information will not fit into a single message) containing final location information according to the *time* IE. A target shallomit sending a *ProvideLocationInformation* if the early location information is not available at the expiration of the time value in the *responseTimeEarlyFix* IE. A server should set the *responseTimeEarlyFix* IE to a value less than that for the *time* IE. A target shall ignore the *responseTimeEarlyFix* IE if its value is not less than that for the *time* IE.  - ***unit*** indicates the unit of the *time* and *responseTimeEarlyFix* fields. Enumerated value '*ten-seconds*' corresponds to a resolution of 10 seconds. Enumerated value '*ten-milli-seconds*' corresponds to a resolution of 0.01 seconds. If this field is absent, the unit/resolution is 1 second. Enumerated value '*ten-milli-seconds*' is only applicable for NR E-CID Positioning, NR DL-TDOA Positioning, NR DL-AoD Positioning, and NR Multi-RTT Positioning. If the enumerated value '*ten-milli-seconds*' is included for methods others than NR E-CID Positioning, NR DL-TDOA Positioning, NR DL-AoD Positioning, and NR Multi-RTT Positioning the target device shall ignore the *unit* field.  - ***velocityRequest*** indicates whether velocity (or measurements related to velocity) is requested (TRUE) or not (FALSE).  - ***responseTimeNB*** If the *periodicalReporting* IE or *responseTime* IE is included in *CommonIEsRequestLocationInformation*, this field should not be included by the location server and shall be ignored by the target device (if included).  - ***timeNB*** indicates the maximum response time as measured between receipt of the *RequestLocationInformation* and transmission of a *ProvideLocationInformation*. If the *unitNB* field is absent, this is given as an integer number of seconds between 1 and 512. If the *unitNB* field is present, the maximum response time is given in units of 10-seconds, between 10 and 5120 seconds.  - ***responseTimeEarlyFixNB*** indicates the maximum response time as measured between receipt of the *RequestLocationInformation* and transmission of a *ProvideLocationInformation* containing early location measurements or an early location estimate. If the *unitNB* field is absent, this is given as an integer number of seconds between 1 and 512. If the *unitNB* field is present, the maximum response time is given in units of 10-seconds, between 10 and 5120 seconds. When this IE is included, a target should send a *ProvideLocationInformation* (or more than one *ProvideLocationInformation* if location information will not fit into a single message) containing early location information according to the *responseTimeEarlyFixNB* IE and a subsequent *ProvideLocationInformation* (or more than one *ProvideLocationInformation* if location information will not fit into a single message) containing final location information according to the *timeNB* IE. A target shall omit sending a *ProvideLocationInformation* if the early location information is not available at the expiration of the time value in the *responseTimeEarlyFixNB* IE. A server should set the *responseTimeEarlyFixNB* IE to a value less than that for the *timeNB* IE. A target shall ignore the *responseTimeEarlyFixNB* IE if its value is not less than that for the *timeNB* IE.  - ***unitNB*** indicates the unit of the *timeNB* and *responseTimeEarlyFixNB* fields. Enumerated value '*ten-second*' corresponds to a resolution of 10 seconds. If this field is absent, the unit/resolution is 1 second.  - ***horizontalAccuracyExt*** indicates the maximum horizontal error in the location estimate at an indicated confidence level. The '*accuracyExt*' corresponds to the encoded high accuracy uncertainty as defined in TS 23.032 [15] and 'confidence' corresponds to confidence as defined in TS 23.032 [15]. This field should not be included by the location server and shall be ignored by the target device if the *horizontalAccuracy* field is included in QoS.  - ***verticalAccuracyExt*** indicates the maximum vertical error in the location estimate at an indicated confidence level and is only applicable when a vertical coordinate is requested. The '*accuracyExt*' corresponds to the encoded high accuracy uncertainty as defined in TS 23.032 [15] and '*confidence*' corresponds to confidence as defined in TS 23.032 [15]. This field should not be included by the location server and shall be ignored by the target device if the *verticalAccuracy* field is included in QoS.  All QoS requirements shall be obtained by the target device to the degree possible but it is permitted to return a response that does not fulfill all QoS requirements if some were not attainable. The single exception is *time* and *timeNB* which shall always be fulfilled – even if that means not fulfilling other QoS requirements.  A target device supporting NB-IoT access shall support the *responseTimeNB* IE*.*  A target device supporting HA GNSS shall support the *HorizontalAccuracyExt*, *VerticalAccuracyEx*, and *unit* fields with enumerated value '*ten-seconds*'.  A target device supporting NB-IoT access and HA GNSS shall support the *unitNB* field. |
| ***environment***  This field provides the target device with information about expected multipath and non line of sight (NLOS) in the current area. The following values are defined:  - badArea: possibly heavy multipath and NLOS conditions (e.g. bad urban or urban).  - notBadArea: no or light multipath and usually LOS conditions (e.g. suburban or rural).  - mixedArea: environment that is mixed or not defined.  If this field is absent, a default value of 'mixedArea' applies. |
| ***locationCoordinateTypes***  This field provides a list of the types of location estimate that the target device may return when a location estimate is obtained by the target. |
| ***velocityTypes***  This fields provides a list of the types of velocity estimate that the target device may return when a velocity estimate is obtained by the target. |
| ***messageSizeLimitNB***  This field provides an octet limit on the amount of location information a target device can return.  - ***measurementLimit*** indicates the maximum amount of location information the target device should return in response to the *RequestLocationInformation* message received from the location server. The limit applies to the overall size of the LPP message at LPP level (LPP Provide Location Information), and is specified in steps of 100 octets. The message size limit is then given by the value provided in *measurementLimit* times 100 octets. |
| ***segmentationInfo***  This field indicates whether this *RequestLocationInformation* message is one of many segments, as specified in clause 4.3.5 |
| ***scheduledLocationTime***  This field indicates that the target device is requested to obtain location measurements or location estimate valid at the *scheduledLocationTime* *T* and comprises the following subfields:  - ***utcTime*** provides *T* in UTC in the form of YYMMDDhhmmssZ.  - ***gnssTime*** provides *T* in GNSS system time of the GNSS indicated by *gnss-TimeID*.  - ***gnss-TOD-msec*** specifies the GNSS TOD in 1-milli-second resolution rounded down to the nearest millisecond unit.  - ***networkTime*** provides *T* in E-UTRA or NR network time.  - ***lte-PhysCellId, lte-ArfcnEUTRA, lte-CellGlobalId*** identifies the reference cell (E-UTRA) that is used for the network time.  - ***lte-systemFrameNumber*** specifies the system frame number in E-UTRA.  - ***nr-PhysCellID***, ***nr-ARFCN*** , ***nr-CellGlobalID*** identifies the reference cell (NR) that is used for the network time.  - ***nr-SFN*** specifies the system frame number in NR.  - ***nr-Slot*** specifies the slot number in NR for the indicated subcarrier spacing (SCS). The total NR network time is given by *nr-SFN* + *nr-Slot*.  - ***relativeTime*** provides *T* in seconds from current time, where current time is defined as the time the *CommonIEsRequestLocationInformation* was received.  NOTE 1: A location estimate returned to an LCS Client, AF or UE for a scheduled location time can be treated by the LCS Client, AF or UE as an estimate of the location of the UE at the scheduled location time (see TS 23.273 [42]).  NOTE 2: If this field is present, at least one of *utcTime*, *gnssTime*, *networkTime,* or *relativeTime* shall be present. |
| ***targetIntegrityRisk***  This field indicates the TIR for which the PL is requested. The TIR is calculated by *P*=10-0.1*n* [hour-1] where *n* is the value of *targetIntegrityRisk* and the range is 10-1 to 10-9 per hour. |
| ***periodicalReportingExt***  This field indicates that extended periodic reporting is requested and comprises the below subfields. If this field is present, the field *periodicalReporting* is absent. Measurement reports containing no measurements or no location estimate are required when a *reportingIntervalMs* expires before a target device is able to obtain new measurements or obtain a new location estimate.  - ***reportingAmount*** indicates the number of periodic location information reports requested. Enumerated values correspond to 2, 4, 8, 16, 32, 64, or infinite/indefinite number of reports. If the *reportingAmount* is '*infinite/indefinite*', the target device should continue periodic reporting until an LPP *Abort* message is received.  - ***reportingIntervalMs*** indicates the interval between location information reports and the response time requirement for the first location information report in milliseconds. |

#### – *CommonIEsProvideLocationInformation*

The *CommonIEsProvideLocationInformation* carries common IEs for a Provide Location Information LPP message Type.

-- ASN1START

CommonIEsProvideLocationInformation ::= SEQUENCE {

locationEstimate LocationCoordinates OPTIONAL,

velocityEstimate Velocity OPTIONAL,

locationError LocationError OPTIONAL,

...,

[[ earlyFixReport-r12 EarlyFixReport-r12 OPTIONAL

]],

[[ locationSource-r13 LocationSource-r13 OPTIONAL,

locationTimestamp-r13 UTCTime OPTIONAL

]],

[[

segmentationInfo-r14 SegmentationInfo-r14 OPTIONAL -- Cond Segmentation

]],

[[

integrityInfo-r17 IntegrityInfo-r17 OPTIONAL

]]

}

LocationCoordinates ::= CHOICE {

ellipsoidPoint Ellipsoid-Point,

ellipsoidPointWithUncertaintyCircle Ellipsoid-PointWithUncertaintyCircle,

ellipsoidPointWithUncertaintyEllipse EllipsoidPointWithUncertaintyEllipse,

polygon Polygon,

ellipsoidPointWithAltitude EllipsoidPointWithAltitude,

ellipsoidPointWithAltitudeAndUncertaintyEllipsoid

EllipsoidPointWithAltitudeAndUncertaintyEllipsoid,

ellipsoidArc EllipsoidArc,

...,

highAccuracyEllipsoidPointWithUncertaintyEllipse-v1510

HighAccuracyEllipsoidPointWithUncertaintyEllipse-r15,

highAccuracyEllipsoidPointWithAltitudeAndUncertaintyEllipsoid-v1510

HighAccuracyEllipsoidPointWithAltitudeAndUncertaintyEllipsoid-r15,

ha-EllipsoidPointWithScalableUncertaintyEllipse-v1680 HA-EllipsoidPointWithScalableUncertaintyEllipse-r16,

ha-EllipsoidPointWithAltitudeAndScalableUncertaintyEllipsoid-v1680

HA-EllipsoidPointWithAltitudeAndScalableUncertaintyEllipsoid-r16,

local2dPointWithUncertaintyEllipse-v1800 Local2dPointWithUncertaintyEllipse-r18,

local3dPointWithUncertaintyEllipsoid-v1800 Local3dPointWithUncertaintyEllipsoid-r18

}

Velocity ::= CHOICE {

horizontalVelocity HorizontalVelocity,

horizontalWithVerticalVelocity HorizontalWithVerticalVelocity,

horizontalVelocityWithUncertainty HorizontalVelocityWithUncertainty,

horizontalWithVerticalVelocityAndUncertainty

HorizontalWithVerticalVelocityAndUncertainty,

...

}

LocationError ::= SEQUENCE {

locationfailurecause LocationFailureCause,

...

}

LocationFailureCause ::= ENUMERATED {

undefined,

requestedMethodNotSupported,

positionMethodFailure,

periodicLocationMeasurementsNotAvailable,

...

}

EarlyFixReport-r12 ::= ENUMERATED {

noMoreMessages,

moreMessagesOnTheWay

}

LocationSource-r13 ::= BIT STRING { a-gnss (0),

wlan (1),

bt (2),

tbs (3),

sensor (4),

ha-gnss-v1510 (5),

motion-sensor-v1550 (6),

dl-tdoa-r16 (7),

dl-aod-r16 (8),

nr-AI-ML-r19 (9)

} (SIZE(1..16))

IntegrityInfo-r17 ::= SEQUENCE {

horizontalProtectionLevel-r17 INTEGER (0..50000),

verticalProtectionLevel-r17 INTEGER (0..50000) OPTIONAL,

achievableTargetIntegrityRisk-r17 INTEGER (10..90) OPTIONAL,

...

}

-- ASN1STOP

| Conditional presence | Explanation |
| --- | --- |
| *Segmentation* | This field is optionally present, need OP, if *lpp-message-segmentation-req* has been received from the location server with bit 1 (*targetToServer*) set to value 1. The field shall be omitted if *lpp‑message‑segmentation-req* has not been received in this location session, or has been received with bit 1 (*targetToServer*) set to value 0. |

| *CommonIEsProvideLocationInformation* field descriptions |
| --- |
| ***locationEstimate***  This field provides a location estimate using one of the geographic shapes defined in TS 23.032 [15]. Coding of the values of the various fields internal to each geographic shape follow the rules in TS 23.032 [15]. The conditions for including this field are defined for the *locationInformationType* field in a Request Location Information message.  NOTE: If the *locationInformationType* field in a Request Location Information message was set to '*locationEstimateAndMeasurementsRequired*' and this field is absent, it means that the PRU location is not available. |
| ***velocityEstimate***  This field provides a velocity estimate using one of the velocity shapes defined in TS 23.032 [15]. Coding of the values of the various fields internal to each velocity shape follow the rules in TS 23.032 [15]. |
| ***locationError***  This field shall be included if and only if a location estimate and measurements are not included in the LPP PDU. The field includes information concerning the reason for the lack of location information. The *LocationFailureCause* '*periodicLocationMeasurementsNotAvailable*' shall be used by the target device if periodic location reporting was requested, but no measurements or location estimate are available when *the reportingInterval* expired. |
| ***earlyFixReport***  This field shall be included if and only if the *ProvideLocationInformation* message contains early location measurements or an early location estimate. The target device shall set the values of this field as follows:  - noMoreMessages: This is the only or last *ProvideLocationInformation* message used to deliver the entire set of early location information.  - moreMessagesOnTheWay: This is one of multiple *ProvideLocationInformation* messages used to deliver the entire set of early location information (if early location information will not fit into a single message).  If this field is included, the IE *SegmentationInfo* shall not be included. |
| ***locationSource***  This field provides the source positioning technology for the location estimate.  NOTE 1: In this version of the specification, the entry 'tbs' is used only for TBS positioning based on MBS signals.  NOTE 2: The entry 'sensor' is used only for positioning technology that uses barometric pressure sensor. The entry 'motion-sensor' is used for positioning technology that uses sensor(s) to detect displacement and movement, e.g. accelerometers, gyros, magnetometers. |
| ***locationTimestamp***  This field provides the UTC time when the location estimate is valid and should take the form of *YYMMDDhhmmssZ*. |
| ***segmentationInfo***  This field indicates whether this *ProvideLocationInformation* message is one of many segments, as specified in clause 4.3.5 |
| ***integrityInfo***  This field provides the integrity result for the *locationEstimate.*  - ***horizontalProtectionLevel*** provides the HPL for the *locationEstimate* along the semi-major axis of the error ellipse. Scale factor 0.01 metre; range 0 – 500 metres.  - ***verticalProtectionLevel*** provides the VPL for the *locationEstimate*. Scale factor 0.01 metre; range 0 – 500 metres.  - ***achievableTargetIntegrityRisk*** indicates the achievable TIR for which the HPL and VPL are provided. The achievable TIR is given by *P*=10-0.1n [hour-1] where *n* is the value of *achievableTargetIntegrityRisk* and the range is 10-1 to 10-9 per hour. If this field is absent, the achievable TIR is the same as the *targetIntegrityRisk* in *CommonIEsRequestLocationInformation*. |

NOTE: Void.

#### *– CommonIEsAbort*

The *CommonIEsAbort* carries common IEs for an Abort LPP message Type.

-- ASN1START

CommonIEsAbort ::= SEQUENCE {

abortCause ENUMERATED {

undefined,

stopPeriodicReporting,

targetDeviceAbort,

networkAbort,

...,

stopPeriodicAssistanceDataDelivery-v1510

}

}

-- ASN1STOP

| *CommonIEsAbort* field descriptions |
| --- |
| ***abortCause***  This IE defines the request to abort an ongoing procedure. The abort cause '*stopPeriodicReporting*' should be used by the location server to stop any ongoing location reporting configured as *periodicalReporting* or *triggeredReporting* in the *CommonIEsRequestLocationInformation*.  The abort cause '*stopPeriodicAssistanceDataDelivery*' should be used by the location server or target device to stop any ongoing periodic assistance data delivery, as specified in clauses 5.2.1a and 5.2.2a. |

#### – *CommonIEsError*

The *CommonIEsError* carries common IEs for an Error LPP message Type.

-- ASN1START

CommonIEsError ::= SEQUENCE {

errorCause ENUMERATED {

undefined,

lppMessageHeaderError,

lppMessageBodyError,

epduError,

incorrectDataValue,

...,

lppSegmentationError-v1450

}

}

-- ASN1STOP

| *CommonIEsError* field descriptions |
| --- |
| *errorCause*  This IE defines the cause for an error. '*lppMessageHeaderError*', '*lppMessageBodyError*' and '*epduError*' is used if a receiver is able to detect a coding error in the LPP header (i.e., in the common fields), LPP message body or in an EPDU, respectively. '*incorrectDataValue*' is used if a receiver receives an incorrect data value. '*lppSegmentationError*' is used if a receiver detects an error in LPP message segmentation. |

### 6.4.3 Common NR Positioning Information Elements

#### – *AreaID-CellList*

The IE *AreaID-CellList* provides the NR Cell-IDs of the TRPs belonging to a particular network area where the associated assistance data are valid. Each cell is included in only one area.

-- ASN1START

AreaID-CellList-r17 ::= SEQUENCE (SIZE(1..maxCellIDsPerArea-r17)) OF NR-Cell-IDs-r17

NR-Cell-IDs-r17 ::= SEQUENCE {

nr-CellGlobalID-r17 NCGI-r15 OPTIONAL, -- Need ON

nr-PhysCellID-r17 NR-PhysCellID-r16 OPTIONAL, -- Need ON

nr-ARFCN-r17 ARFCN-ValueNR-r15 OPTIONAL, -- Need ON

...

}

-- ASN1STOP

| *AreaID-CellList* field descriptions |
| --- |
| ***nr-CellGlobalID***  This field specifies the NR Cell Global ID of the TRP belonging to a particular network area where the associated assistance data are applicable. |
| ***nr-PhysCellID***  This field specifies the physical cell identity of the TRP belonging to a particular network area where the associated assistance data are applicable. |
| ***nr-ARFCN***  This field specifies the NR-ARFCN of the TRP's CD-SSB (as defined in TS 38.300 [47]) corresponding to *nr-PhysCellID*. |

#### – *DL-PRS-ID-Info*

The IE *DL-PRS-ID-Info* provides the IDs of the reference TRPs' DL-PRS Resources.

-- ASN1START

DL-PRS-ID-Info-r16 ::= SEQUENCE {

dl-PRS-ID-r16 INTEGER (0..255),

nr-DL-PRS-ResourceID-List-r16 SEQUENCE (SIZE (1..nrMaxResourceIDs-r16)) OF

NR-DL-PRS-ResourceID-r16

OPTIONAL, -- Need ON

nr-DL-PRS-ResourceSetID-r16 NR-DL-PRS-ResourceSetID-r16

OPTIONAL -- Need ON

}

-- ASN1STOP

| *DL-PRS-ID-Info* field descriptions |
| --- |
| ***nr-DL-PRS-ResourceID-List***  This field provides a list of DL-PRS Resource IDs under the same DL-PRS Resource Set. |

#### – *LCS-GCS-TranslationParameter*

The IE *LCS-GCS-TranslationParameter* provides the angles α (bearing angle), β (downtilt angle) and γ (slant angle) for the translation of a Local Coordinate System (LCS) to a Global Coordinate System (GCS) as defined in TR 38.901 [44].

-- ASN1START

LCS-GCS-TranslationParameter-r16 ::= SEQUENCE {

alpha-r16 INTEGER (0..359),

alpha-fine-r16 INTEGER (0..9) OPTIONAL, -- Cond AzElFine

beta-r16 INTEGER (0..359),

beta-fine-r16 INTEGER (0..9) OPTIONAL, -- Cond AzElFine

gamma-r16 INTEGER (0..359),

gamma-fine-r16 INTEGER (0..9) OPTIONAL, -- Cond AzElFine

...

}

-- ASN1STOP

| Conditional presence | Explanation |
| --- | --- |
| *AzElFine* | The field is mandatory present if the angles where this IE is used are provided with 0.1 degrees resolution; otherwise it is not present. |

|  |
| --- |
| *LCS-GCS-TranslationParameter* field descriptions |
| ***alpha***  This field specifies the bearing angle α for the translation of the LCS to a GCS as defined in TR 38.901 [44].  Scale factor 1 degree; range 0 to 359 degrees. |
| ***alpha-fine***  This field provides finer granularity for the *alpha*.  The total bearing angle α is given by *alpha* + *alpha-fine.*  Scale factor 0.1 degrees; range 0 to 0.9 degrees. |
| ***beta***  This field specifies the downtilt angle β for the translation of the LCS to a GCS as defined in TR 38.901 [44].  Scale factor 1 degree; range 0 to 359 degrees. |
| ***beta-fine***  This field provides finer granularity for the *beta*.  The total downtilt angle β is given by *beta* + *beta-fine.*  Scale factor 0.1 degrees; range 0 to 0.9 degrees. |
| ***gamma***  This field specifies the slant angle γ for the translation of the LCS to a GCS as defined in TR 38.901 [44].  Scale factor 1 degree; range 0 to 359 degrees. |
| ***gamma-fine***  This field provides finer granularity for the *gamma*.  The total slant angle γ is given by *gamma* + *gamma-fine.*  Scale factor 0.1 degrees; range 0 to 0.9 degrees. |

#### – *LocalOrigin*

The IE *LocalOrigin* is used to indicate a reference point and optionally a horizontal orientation that defines the origin and horizontal orientation of a local Cartesian Coordinate System as defined in TS 23.032 [15].

-- ASN1START

LocalOrigin-r18 ::= SEQUENCE {

coordinateID-r18 VisibleString (SIZE (1..256)),

point-r18 HighAccuracyEllipsoidPointWithAltitudeAndUncertaintyEllipsoid-r15 OPTIONAL, -- Need ON

horizAxesOrientation-r18 INTEGER (0..3599) OPTIONAL, -- Need ON

...

}

-- ASN1STOP

|  |
| --- |
| *LocalOrigin* field descriptions |
| ***coordinateID***  This field defines a known reference point which is configured by the PLMN operator. |
| ***point***  This field specifies geodetic coordinate with uncertainty of the local origin. |
| ***horizAxesOrientation***  This field specifies the local coordinate system horizontal orientation angle clockwise from northing. Scale factor 0.1 degrees. |

#### – *LOS-NLOS-Indicator*

The IE *LOS-NLOS-Indicator* provides information on the likelihood of a Line-of-Sight (LOS) propagation path from the source to the receiver.

-- ASN1START

LOS-NLOS-Indicator-r17 ::= SEQUENCE {

indicator-r17 CHOICE {

soft-r17 INTEGER (0..10),

hard-r17 BOOLEAN

},

...

}

-- ASN1STOP

| *LOS-NLOS-Indicator* field descriptions |
| --- |
| ***indicator***  This field provides information on the likelihood of a Line-of-Sight propagation path from the source to the receiver with a value of 1 corresponding to LoS and a value of 0 corresponding to NLoS.  - ***soft***: Integer value '0' indicates likelihood 0, integer value '10' indicates likelihood 1. Scale factor 0.1; range 0 to 1.  - ***hard***: FALSE indicates likelihood '0', TRUE indicates likelihood '1'. |

#### – *LOS-NLOS-IndicatorGranularity1*

The IE *LOS-NLOS-IndicatorGranularity1* provides information on the *LOS-NLOS-Indicator* granularity.

-- ASN1START

LOS-NLOS-IndicatorGranularity1-r17 ::= ENUMERATED { trpspecific, resourcespecific }

-- ASN1STOP

#### – *LOS-NLOS-IndicatorGranularity2*

The IE *LOS-NLOS-IndicatorGranularity2* provides information on the *LOS-NLOS-Indicator* granularity.

-- ASN1START

LOS-NLOS-IndicatorGranularity2-r17 ::= ENUMERATED { trpspecific, resourcespecific, both }

-- ASN1STOP

#### – *LOS-NLOS-IndicatorType1*

The IE *LOS-NLOS-IndicatorType1* provides information on the *LOS-NLOS-Indicator* type that is requested by the location server.

-- ASN1START

LOS-NLOS-IndicatorType1-r17 ::= ENUMERATED { hardvalue, softvalue }

-- ASN1STOP

#### – *LOS-NLOS-IndicatorType2*

The IE *LOS-NLOS-IndicatorType2* provides information on the *LOS-NLOS-Indicator* type that is supported by the target device.

-- ASN1START

LOS-NLOS-IndicatorType2-r17 ::= ENUMERATED { hardvalue, hardAndsoftvalue }

-- ASN1STOP

#### *– NR-AdditionalPathList*

The IE *NR-AdditionalPathList* is used by the target device to provide information about additional paths in association to the TOA measurements associated to NR positioning in the form of a relative time difference and a quality value. The additional path *nr-RelativeTimeDifference* is the detected path timing relative to the detected path timing used for the TOA value, and each additional path can be associated with a quality value *nr-PathQuality.*

-- ASN1START

NR-AdditionalPathList-r16 ::= SEQUENCE (SIZE(1..2)) OF NR-AdditionalPath-r16

NR-AdditionalPathListExt-r17 ::= SEQUENCE (SIZE(1..8)) OF NR-AdditionalPath-r16

NR-AdditionalPath-r16 ::= SEQUENCE {

nr-RelativeTimeDifference-r16 CHOICE {

k0-r16 INTEGER(0..16351),

k1-r16 INTEGER(0..8176),

k2-r16 INTEGER(0..4088),

k3-r16 INTEGER(0..2044),

k4-r16 INTEGER(0..1022),

k5-r16 INTEGER(0..511),

...,

kMinus6-r18 INTEGER(0..1046401),

kMinus5-r18 INTEGER(0..523201),

kMinus4-r18 INTEGER(0..261601),

kMinus3-r18 INTEGER(0..130801),

kMinus2-r18 INTEGER(0..65401),

kMinus1-r18 INTEGER(0..32701)

},

nr-PathQuality-r16 NR-TimingQuality-r16 OPTIONAL,

...,

[[

nr-DL-PRS-RSRPP-r17 INTEGER (0..126) OPTIONAL

]]

}

-- ASN1STOP

| *NR-AdditionalPathList* field descriptions |
| --- |
| ***nr-RelativeTimeDifference***  This field specifies the additional detected path timing relative to the detected path timing of the reference resource. The mapping of reported values and measured quantity value is defined in TS 38.133 [46] clause 10.1.23.3.3 and 10.1.25.3.3. A positive value indicates that the particular path is later in time than the detected path of the reference; a negative value indicates that the particular path is earlier in time than the detected path of the reference. |
| ***nr-PathQuality***  This field specifies the target device′s best estimate of the quality of the detected timing of the additional path. |
| ***nr-DL-PRS-RSRPP***  This field specifies the DL-PRS reference signal received path power (DL PRS-RSRPP) of the *NR-AdditionalPath* reported, as defined in TS 38.215 [36]. The mapping of the quantity is defined as in TS 38.133 [46]. |

#### *– NR-AggregatedDL-PRS-ResourceInfo-Element*

The IE *NR-AggregatedDL-PRS-ResourceInfo-Element* is used by the target device to indicate each of the aggregated DL-PRS Resource Set and/or the DL-PRS Resource to the location server.

-- ASN1START

NR-AggregatedDL-PRS-ResourceInfo-Element-r18 ::= SEQUENCE {

aggregatedDL-PRS-ID-r18 INTEGER (0..255) OPTIONAL,

nr-DL-PRS-ResourceSetID-r18 NR-DL-PRS-ResourceSetID-r16 OPTIONAL,

nr-DL-PRS-ResourceID-r18 NR-DL-PRS-ResourceID-r16 OPTIONAL,

...

}

-- ASN1STOP

#### – *NR-DL-PRS-AssistanceData*

The IE *NR-DL-PRS-AssistanceData* is used by the location server to provide DL-PRS assistance data.

NOTE 1: The location server should include at least one TRP for which the SFN can be obtained by the target device, e.g. the serving TRP.

NOTE 2: The *nr-DL-PRS-ReferenceInfo* defines the "assistance data reference" TRP whose DL-PRS configuration is included in *nr-DL-PRS-AssistanceDataList*. The *nr-DL-PRS-SFN0-Offset's* and *nr-DL-PRS-expectedRSTD's* in *nr-DL-PRS-AssistanceDataList* are provided relative to the "assistance data reference" TRP.

NOTE 3: The network signals a value of zero for the *nr-DL-PRS-SFN0-Offset*, *nr-DL-PRS-expectedRSTD*, and *nr-DL-PRS-expectedRSTD-uncertainty* of the "assistance data reference" TRP in *nr-DL-PRS-AssistanceDataList*.

NOTE 4: For NR DL-TDOA positioning (see clause 6.5.10) the *nr-DL-PRS-ReferenceInfo* defines also the requested "RSTD reference".

For DL-PRS processing, the LPP layer may inform lower layers to start performing DL-PRS measurements and provide to lower layers the information about the location of DL-PRS, e.g. DL-PRS-PointA, DL-PRS Positioning occasion information.

-- ASN1START

NR-DL-PRS-AssistanceData-r16 ::= SEQUENCE {

nr-DL-PRS-ReferenceInfo-r16 DL-PRS-ID-Info-r16,

nr-DL-PRS-AssistanceDataList-r16 SEQUENCE (SIZE (1..nrMaxFreqLayers-r16)) OF

NR-DL-PRS-AssistanceDataPerFreq-r16,

nr-SSB-Config-r16 SEQUENCE (SIZE (1..nrMaxTRPs-r16)) OF

NR-SSB-Config-r16 OPTIONAL, -- Need ON

...,

[[

nr-DL-PRS-AggregationInfo-r18 NR-DL-PRS-AggregationInfo-r18 OPTIONAL -- Need ON

]]

}

NR-DL-PRS-AssistanceDataPerFreq-r16 ::= SEQUENCE {

nr-DL-PRS-PositioningFrequencyLayer-r16

NR-DL-PRS-PositioningFrequencyLayer-r16,

nr-DL-PRS-AssistanceDataPerFreq-r16 SEQUENCE (SIZE (1..nrMaxTRPsPerFreq-r16)) OF

NR-DL-PRS-AssistanceDataPerTRP-r16,

...

}

NR-DL-PRS-AssistanceDataPerTRP-r16 ::= SEQUENCE {

dl-PRS-ID-r16 INTEGER (0..255),

nr-PhysCellID-r16 NR-PhysCellID-r16 OPTIONAL, -- Need ON

nr-CellGlobalID-r16 NCGI-r15 OPTIONAL, -- Need ON

nr-ARFCN-r16 ARFCN-ValueNR-r15 OPTIONAL, -- Need ON

nr-DL-PRS-SFN0-Offset-r16 NR-DL-PRS-SFN0-Offset-r16,

nr-DL-PRS-ExpectedRSTD-r16 INTEGER (-3841..3841),

nr-DL-PRS-ExpectedRSTD-Uncertainty-r16

INTEGER (0..246),

nr-DL-PRS-Info-r16 NR-DL-PRS-Info-r16,

...,

[[

prs-OnlyTP-r16 ENUMERATED { true } OPTIONAL -- Need ON

]],

[[

nr-DL-PRS-ExpectedAoD-or-AoA-r17

NR-DL-PRS-ExpectedAoD-or-AoA-r17 OPTIONAL -- Need ON

]]

}

NR-DL-PRS-PositioningFrequencyLayer-r16 ::= SEQUENCE {

dl-PRS-SubcarrierSpacing-r16 ENUMERATED {kHz15, kHz30, kHz60, kHz120, ...},

dl-PRS-ResourceBandwidth-r16 INTEGER (1..63),

dl-PRS-StartPRB-r16 INTEGER (0..2176),

dl-PRS-PointA-r16 ARFCN-ValueNR-r15,

dl-PRS-CombSizeN-r16 ENUMERATED {n2, n4, n6, n12, ...},

dl-PRS-CyclicPrefix-r16 ENUMERATED {normal, extended, ...},

...

}

NR-DL-PRS-SFN0-Offset-r16 ::= SEQUENCE {

sfn-Offset-r16 INTEGER (0..1023),

integerSubframeOffset-r16 INTEGER (0..9),

...

}

NR-DL-PRS-ExpectedAoD-or-AoA-r17 ::= CHOICE {

expectedAoD-r17 SEQUENCE {

expectedDL-AzimuthAoD-r17 INTEGER (0..359),

expectedDL-AzimuthAoD-Unc-r17 INTEGER (0..60) OPTIONAL, -- Need OP

expectedDL-ZenithAoD-r17 INTEGER (0..180),

expectedDL-ZenithAoD-Unc-r17 INTEGER (0..30) OPTIONAL -- Need OP

},

expectedAoA-r17 SEQUENCE {

expectedDL-AzimuthAoA-r17 INTEGER (0..359),

expectedDL-AzimuthAoA-Unc-r17 INTEGER (0..60) OPTIONAL, -- Need OP

expectedDL-ZenithAoA-r17 INTEGER (0..180),

expectedDL-ZenithAoA-Unc-r17 INTEGER (0..30) OPTIONAL -- Need OP

}

}

NR-DL-PRS-AggregationInfo-r18 ::= SEQUENCE (SIZE (1..nrMaxNumPRS-BandWidthAggregation-r18)) OF

NR-linkedDL-PRS-ResourceSetID-PRS-AggregationList-r18

NR-linkedDL-PRS-ResourceSetID-PRS-AggregationList-r18 ::= SEQUENCE (SIZE (2..3)) OF

NR-DL-PRS-AggregationElement-r18

NR-DL-PRS-AggregationElement-r18 ::= SEQUENCE {

nr-DL-PRS-FrequencyLayerIndex-r18 INTEGER (0..nrMaxFreqLayers-1-r16),

nr-DL-PRS-TRP-Index-r18 INTEGER (0..nrMaxTRPsPerFreq-1-r16),

nr-DL-PRS-ResourceSetIndex-r18 INTEGER (0..nrMaxSetsPerTrpPerFreqLayer-1-r16)

}

-- ASN1STOP

|  |
| --- |
| *NR-DL-PRS-AssistanceData* field descriptions |
| ***nr-DL-PRS-ReferenceInfo***  This field specifies the IDs of the assistance data reference TRP. |
| ***nr-DL-PRS-AssistanceDataList***  This field specifies the DL-PRS Resources for each frequency layer. |
| ***nr-SSB-Config***  This field specifies the SSB configuration of the TRPs. |
| ***nr-DL-PRS-AggregationInfo***  This field specifies the DL-PRS Resource Sets across DL-PRS Positioning Frequency Layers available for DL-PRS bandwidth aggregation. The 2 or 3 DL-PRS Resource Sets indicated by IE  *NR-linkedDL-PRS-ResourceSetID-PRS-AggregationList* is linked for bandwidth aggregation.  - ***nr-DL-PRS-FrequencyLayerIndex***: This field indicates the frequency layer provided in *nr-DL-PRS-AssistanceDataList*. Value 0 corresponds to the first frequency layer provided in *nr-DL-PRS-AssistanceDataList*, value 1 to the second frequency layer in *nr-DL-PRS-AssistanceDataList*, and so on.  - ***nr-DL-PRS-TRP-Index***: This field indicates the TRP/DL-PRS ID used for bandwidth aggregation belonging to the *nr-DL-PRS-FrequencyLayerIndex*. Value 0 corresponds to the first TRP/DL-PRS ID provided in *nr-DL-PRS-AssistanceDataPerFreq*, value 1 to the second TRP/DL-PRS ID in *nr-DL-PRS-AssistanceDataPerFreq*, and so on.  - ***nr-DL-PRS-ResourceSetIndex***: This field indicates the DL-PRS Resource Set ID used for bandwidth aggregation belonging to *nr-DL-PRS-TRP-Index*. Value 0 corresponds to the first DL-PRS Resource Set provided in *nr-DL-PRS-ResourceSetList*, value 1 to the second DL-PRS Resource Set in *nr-DL-PRS-ResourceSetList.*  NOTE: The linked DL-PRS Resource Sets from two or three Positioning Frequency Layers in a *NR-linkedDL-PRS-ResourceSetID-PRS-AggregationList* are from the same TRP. |
| ***nr-DL-PRS-PositioningFrequencyLayer***  This field specifies the Positioning Frequency Layer for the *nr-DL-PRS-AssistanceDataPerFreq* field. |
| ***nr-DL-PRS-AssistanceDataPerFreq***  This field specifies the DL-PRS Resources for the TRPs within the Positioning Frequency Layer. |
| ***dl-PRS-ID***  This field is used along with a DL-PRS Resource Set ID and a DL-PRS Resource ID to uniquely identify a DL-PRS Resource, and is associated with a single TRP. |
| ***nr-PhysCellID***  This field specifies the physical cell identity of the TRP. When the field *prs-OnlyTP* is included, this field is not included. |
| ***nr-CellGlobalID***  This field specifies the NCGI, the globally unique identity of a cell in NR, as defined in TS 38.331 [35]. When the field *prs-OnlyTP* is included, this field is not included. |
| ***nr-ARFCN***  This field specifies the NR-ARFCN of the TRP's CD-SSB (as defined in TS 38.300 [47]) corresponding to *nr-PhysCellID*. When the field *prs-OnlyTP* is included, this field is not included. |
| ***nr-DL-PRS-SFN0-Offset***  This field specifies the time offset of the SFN#0 slot#0 for the given TRP with respect to SFN#0 slot#0 of the assistance data reference TRP and comprises the following subfields:  - ***sfn-Offset*** specifies the SFN offset at the TRP antenna location between the assistance data reference TRP and this neighbour TRP.  The offset corresponds to the number of full radio frames counted from the beginning of a radio frame #0 of the assistance data reference TRP to the beginning of the closest subsequent radio frame #0 of this neighbour TRP.  - ***integerSubframeOffset*** specifies the frame boundary offset at the TRP antenna location between the assistance data reference TRP and this neighbour TRP counted in full subframes.  The offset corresponds to the number of full subframes counted from the beginning of a subframe #0 of the assistance data reference TRP to the beginning of the closest subsequent subframe #0 of this neighbour TRP.  NOTE: The location server sets the value in accordance with the defined search window for the target device using *nr-DL-PRS-ExpectedRSTD* and *nr-DL-PRS-ExpectedRSTD-Uncertainty*. |
| ***nr-DL-PRS-ExpectedRSTD***  This field indicates the RSTD value that the target device is expected to measure between this TRP and the assistance data reference TRP. The *nr-DL-PRS-ExpectedRSTD* field takes into account the expected propagation time difference as well as transmit time difference of DL-PRS positioning occasions between the two TRPs. The resolution is 4×Ts, with Ts=1/(15000\*2048) seconds. |
| ***nr-DL-PRS-ExpectedRSTD-Uncertainty***  This field indicates the uncertainty in *nr-DL-PRS-ExpectedRSTD* value.The uncertainty is related to the location server′s a‑priori estimate of the target device location. The *nr-DL-PRS-ExpectedRSTD* and *nr-DL-PRS-ExpectedRSTD-Uncertainty* togetherdefine the search window for the target device.  The resolution R is  - Ts if all DL-PRS Resources are in frequency range 2,  - 4×Ts otherwise,  with Ts=1/(15000\*2048) seconds.  The target device may assume that the beginning of the subframe for the DL-PRS of this TRP is received within the search window of size  - [*-nr-*DL*-PRS-ExpectedRSTD-Uncertainty*×R *;* *nr-DL-PRS-ExpectedRSTD-Uncertainty*×R] centred at TREF*+*1 millisecond×N+*nr-DL-PRS-ExpectedRSTD*×4×Ts,  where TREF is the reception time of the beginning of the subframe for the DL-PRS of the assistance data reference TRP at the target device antenna connector, and N can be calculated based on  - *nr-DL-PRS-SFN0-Offset*  - *dl-PRS-Periodicity-and-ResourceSetSlotOffset*  - *dl-PRS-ResourceSlotOffset.* |
| ***nr-DL-PRS-Info***  This field specifies the DL-PRS configuration of the TRP. |
| ***dl-PRS-SubcarrierSpacing***  This field specifies the subcarrier spacing of the DL-PRS Resource. 15, 30, 60 kHz for FR1; 60, 120 kHz for FR2. All DL-PRS Resources and DL-PRS Resource Sets in the same Positioning Frequency layer have the same value of *dl-PRS-SubcarrierSpacing*. |
| ***dl-PRS-ResourceBandwidth***  This field specifies the number of PRBs allocated for the DL-PRS Resource (allocated DL-PRS bandwidth) in multiples of 4 PRBs. All DL-PRS Resources of the DL-PRS Resource Set have the same bandwidth. All DL-PRS Resource Sets belonging to the same Positioning Frequency Layer have the same value of DL-PRS Bandwidth and Start PRB.  Integer value 1 corresponds to 24 PRBs, value 2 corresponds to 28 PRBs, value 3 corresponds to 32 PRBs and so on. |
| ***dl-PRS-StartPRB***  This field specifies the start PRB index defined as offset with respect to reference DL-PRS Point A for the Positioning Frequency Layer. All DL-PRS Resources Sets belonging to the same Positioning Frequency Layer have the same value of *dl-PRS-StartPRB*. |
| ***dl-PRS-PointA***  This field specifies the absolute frequency of the reference resource block for the DL-PRS. Its lowest subcarrier is also known as DL-PRS Point A. A single DL-PRS Point A for DL-PRS Resource allocation is provided per Positioning Frequency Layer. All DL-PRS Resources belonging to the same DL-PRS Resource Set have the same DL-PRS Point A. |
| ***dl-PRS-CombSizeN***  This field specifies the Resource Element spacing in each symbol of the DL-PRS Resource. All DL-PRS Resource Sets belonging to the same Positioning Frequency Layer have the same value of comb size N. |
| ***dl-PRS-CyclicPrefix***  This field specifies the Cyclic Prefix length of the DL-PRS Resource. All DL-PRS Resources Sets belonging to the same Positioning Frequency Layer have the same value of *dl-PRS-CyclicPrefix*. |
| ***prs-OnlyTP***  This field, if present, indicates that the *NR-DL-PRS-AssistanceData* is provided for a PRS-only TP. Whether the field is present or absent should be the same for all the *NR-DL-PRS-AssistanceData* of all the DL-PRS transmitted under the same TP.  The target device shall not assume that any other signals or physical channels are present for the TRP other than DL-PRS. |
| ***nr-DL-PRS-ExpectedAoD-or-AoA***  This field specifies the expected AoD or AoA in the Global Coordinate System (GCS) at the target device location together with uncertainty.  - ***expectedDL-AzimuthAoD***: This field specifies the expected azimuth angle of departure. Scale factor 1 degree; range 0 to 359 degrees.  - ***expectedDL-AzimuthAoD-Unc***: This field specifies the (single-sided) uncertainty of the expected azimuth angle of departure. If this field is absent, it indicates maximum uncertainty (60 degrees). Scale factor 1 degree; range 0 to 60 degrees.  - ***expectedDL-ZenithAoD***: This field specifies the expected elevation angle of departure. Scale factor 1 degree; range 0 to 180 degrees.  - ***expectedDL-ZenithAoD-Unc***: This field specifies the (single-sided) uncertainty of the expected elevation angle of departure. If this field is absent, it indicates maximum uncertainty (30 degrees). Scale factor 1 degree; range 0 to 30 degrees.  - ***expectedDL-AzimuthAoA***: This field specifies the expected azimuth angle of arrival.  Scale factor 1 degree; range 0 to 359 degrees.  - ***expectedDL-AzimuthAoA-Unc***: This field specifies the (single-sided) uncertainty of the expected azimuth angle of arrival. If this field is absent, it indicates maximum uncertainty (60 degrees). Scale factor 1 degree; range 0 to 60 degrees.  - ***expectedDL-ZenithAoA***: This field specifies the expected elevation angle of arrival.  Scale factor 1 degree; range 0 to 180 degrees.  - ***expectedDL-ZenithAoA-Unc***: This field specifies the (single-sided) uncertainty of the expected elevation angle of arrival. If this field is absent, it indicates maximum uncertainty (30 degrees). Scale factor 1 degree; range 0 to 30 degrees. |

#### – *NR-DL-PRS-BeamInfo*

The IE *NR-DL-PRS-BeamInfo* is used by the location server to provide spatial direction information of the DL-PRS Resources together with integrity information.

-- ASN1START

NR-DL-PRS-BeamInfo-r16 ::= SEQUENCE (SIZE (1..nrMaxFreqLayers-r16)) OF

NR-DL-PRS-BeamInfoPerFreqLayer-r16

NR-DL-PRS-BeamInfoPerFreqLayer-r16 ::= SEQUENCE (SIZE (1..nrMaxTRPsPerFreq-r16)) OF

NR-DL-PRS-BeamInfoPerTRP-r16

NR-DL-PRS-BeamInfoPerTRP-r16 ::= SEQUENCE {

dl-PRS-ID-r16 INTEGER (0..255),

nr-PhysCellID-r16 NR-PhysCellID-r16 OPTIONAL, -- Need ON

nr-CellGlobalID-r16 NCGI-r15 OPTIONAL, -- Need ON

nr-ARFCN-r16 ARFCN-ValueNR-r15 OPTIONAL, -- Need ON

associated-DL-PRS-ID-r16 INTEGER (0..255) OPTIONAL, -- Need OP

lcs-GCS-TranslationParameter-r16 LCS-GCS-TranslationParameter-r16

OPTIONAL, -- Need OP

dl-PRS-BeamInfoSet-r16 DL-PRS-BeamInfoSet-r16 OPTIONAL, -- Need OP

...

}

DL-PRS-BeamInfoSet-r16 ::= SEQUENCE (SIZE(1..nrMaxSetsPerTrpPerFreqLayer-r16)) OF

DL-PRS-BeamInfoResourceSet-r16

DL-PRS-BeamInfoResourceSet-r16 ::= SEQUENCE (SIZE(1..nrMaxResourcesPerSet-r16)) OF

DL-PRS-BeamInfoElement-r16

DL-PRS-BeamInfoElement-r16 ::= SEQUENCE {

dl-PRS-Azimuth-r16 INTEGER (0..359),

dl-PRS-Azimuth-fine-r16 INTEGER (0..9) OPTIONAL, -- Need ON

dl-PRS-Elevation-r16 INTEGER (0..180) OPTIONAL, -- Need ON

dl-PRS-Elevation-fine-r16 INTEGER (0..9) OPTIONAL, -- Need ON

...,

[[

nr-IntegrityBeamInfoBounds-r18 NR-IntegrityBeamInfoBounds-r18 OPTIONAL -- Need OP

]]

}

NR-IntegrityBeamInfoBounds-r18 ::= SEQUENCE {

meanAzimuth-r18 INTEGER (0..255),

stdDevAzimuth-r18 INTEGER (0..255),

meanElevation-r18 INTEGER (0..255),

stdDevElevation-r18 INTEGER (0..255),

...

}

-- ASN1STOP

| *NR-DL-PRS-BeamInfo* field descriptions |
| --- |
| ***dl-PRS-ID***  This field is used along with a DL-PRS Resource Set ID and a DL-PRS Resources ID to uniquely identify a DL-PRS Resource. This ID can be associated with multiple DL-PRS Resource Sets associated with a single TRP.  Each TRP should only be associated with one such ID. |
| ***nr-PhysCellID***  This field specifies the physical cell identity of the associated TRP, as defined in TS 38.331 [35]. |
| ***nr-CellGlobalID***  This field specifies the NCGI, the globally unique identity of a cell in NR, of the associated TRP, as defined in TS 38.331 [35]. The server should include this field if it considers that it is needed to resolve ambiguity in the TRP indicated by *nr-PhysCellID*. |
| ***nr-ARFCN***  This field specifies the NR-ARFCN of the TRP's CD-SSB (as defined in TS 38.300 [47]) corresponding to *nr-PhysCellID*. |
| ***associated-DL-PRS-ID***  This field specifies the *dl-PRS-ID* of the associated TRP from which the beam information is obtained. See the field descriptions of *dl-PRS-BeamInfoSet* and *lcs-GCS-TranslationParameter*. |
| ***lcs-GCS-TranslationParameter***  This field provides the angles α (bearing angle), β (downtilt angle) and γ (slant angle) for the translation of a Local Coordinate System (LCS) to a Global Coordinate System (GCS) as defined in TR 38.901 [44]. If this field and the field *associated-DL-PRS-ID* are absent, the *dl-PRS-Azimuth* and *dl-PRS-Elevation* are provided in a GCS. If this field is absent and the *associated-DL-PRS-ID field* is present, then the *lcs-GCS-TranslationParameter* for this TRP is obtained from the *lcs-GCS-TranslationParameter* of the associated TRP. |
| ***dl-PRS-BeamInfoSet***  This field provides the DL-PRS beam information for each DL-PRS Resource of the DL-PRS Resource Set associated with this TRP. If this field is absent and the field *associated-DL-PRS-ID* is present, the *dl-PRS-BeamInfoSet* for this TRP are obtained from the *dl-PRS-BeamInfoSet* of the associated TRP. |
| ***dl-PRS-Azimuth***  This field specifies the azimuth angle of the boresight direction in which the DL-PRS Resources associated with this DL-PRS Resource ID in the DL-PRS Resource Set are transmitted.  For a Global Coordinate System (GCS), the azimuth angle is measured counter-clockwise from geographical North.  For a Local Coordinate System (LCS), the azimuth angle is measured measured counter-clockwise from the x-axis of the LCS.  Scale factor 1 degree; range 0 to 359 degrees. |
| ***dl-PRS-Azimuth-fine***  This field provides finer granularity for the *dl-PRS-Azimuth*.  The total azimuth angle of the boresight direction is given by *dl-PRS-Azimuth* + *dl-PRS-Azimuth-fine.*  Scale factor 0.1 degrees; range 0 to 0.9 degrees. |
| ***dl-PRS-Elevation***  This field specifies the elevation angle of the boresight direction in which the DL-PRS Resources associated with this DL-PRS Resource ID in the DL-PRS Resource Set are transmitted.  For a Global Coordinate System (GCS), the elevation angle is measured relative to zenith and positive to the horizontal direction (elevation 0 deg. points to zenith, 90 deg to the horizon).  For a Local Coordinate System (LCS), the elevation angle is measured relative to the z-axis of the LCS (elevation 0 deg. points to the z-axis, 90 deg to the x-y plane).  Scale factor 1 degree; range 0 to 180 degrees. |
| ***dl-PRS-Elevation-fine***  This field provides finer granularity for the *dl-PRS-Elevation*.  The total elevation angle of the boresight direction is given by *dl-PRS-Elevation* + *dl-PRS-Elevation-fine.*  Scale factor 0.1 degrees; range 0 to 0.9 degrees. |
| ***nr-IntegrityBeamInfoBounds***  This field provides an overbounding model that bounds the spatial direction information of the DL-PRS Resources. If this field is absent, the *nr-IntegrityBeamInfoBounds* of this instance of the *DL-PRS-BeamInfoElement* is the same as the *nr-IntegrityBeamInfoBounds* of the previous instance of the *DL-PRS-BeamInfoElement* in *DL-PRS-BeamInfoResourceSet*. If integrity bounds are provided, this field shall be present at least in the first instance of the *DL-PRS-BeamInfoResourceSet*. It comprises the following sub-fields:  - ***meanAzimuth***: This field specifies the mean azimuth error bound which is the mean value for an overbounding model that bounds the azimuth angle error of the boresight direction in which the DL-PRS Resources associated with this DL-PRS Resource ID in the DL-PRS Resource Set are transmitted. The bound is *meanAzimuth* + K \* *stdDevAzimuth* and shall be so that the probability of it to be exceeded shall be lower than IRallocation for *ir-Minimum* < IRallocation < *ir-Maximum*, where K = normInv(IRallocation / 2) and *ir-Minimum*, *ir-Maximum* as provided in IE *NR-IntegrityServiceParameters*. This IRallocation is a fraction of the Target Integrity Risk that represents the integrity risk budget available.  Scale factor 0.1 degrees; range 0-25.5 degrees.  - ***stdDevAzimuth***: This field specifies the standard deviation azimuth error bound which is the standard deviation for an overbounding model that bounds the azimuth error of the boresight direction in which the DL-PRS Resources associated with this DL-PRS Resource ID in the DL-PRS Resource Set are transmitted.  Scale factor 0.1 degrees; range 0-25.5 degrees.  - ***meanElevation***: This field specifies the mean elevation error bound which is the mean value for an overbounding model that bounds the elevation angle error of the boresight direction in which the DL-PRS Resources associated with this DL-PRS Resource ID in the DL-PRS Resource Set are transmitted. The bound is *meanElevation* + K \* *stdDevElevation* and shall be so that the probability of it to be exceeded shall be lower than IRallocation for *ir-Minimum* < IRallocation < *ir-Maximum*, where K = normInv(IRallocation / 2) and *ir-Minimum*, *ir-Maximum* as provided in IE *NR-IntegrityServiceParameters*. This IRallocation is a fraction of the Target Integrity Risk that represents the integrity risk budget available.  Scale factor 0.1 degrees; range 0-25.5 degrees.  - ***stdDevElevation***: This field specifies the standard deviation elevation error bound which is the standard deviation for an overbounding model that bounds the elevation error of the boresight direction in which the DL-PRS Resources associated with this DL-PRS Resource ID in the DL-PRS Resource Set are transmitted.  Scale factor 0.1 degrees; range 0-25.5 degrees. |

#### – *NR-DL-PRS-ExpectedLOS-NLOS-Assistance*

The IE *NR-DL-PRS-ExpectedLOS-NLOS-Assistance* is used by the location server to provide the expected likelihood of a LOS propagation path from a TRP to the target device, or for all DL-PRS Resources of the TRP to the target device.

-- ASN1START

NR-DL-PRS-ExpectedLOS-NLOS-Assistance-r17 ::= SEQUENCE (SIZE (1..nrMaxFreqLayers-r16)) OF

NR-DL-PRS-ExpectedLOS-NLOS-AssistancePerFreqLayer-r17

NR-DL-PRS-ExpectedLOS-NLOS-AssistancePerFreqLayer-r17 ::=

SEQUENCE (SIZE (1..nrMaxTRPsPerFreq-r16)) OF

NR-DL-PRS-ExpectedLOS-NLOS-AssistancePerTRP-r17

NR-DL-PRS-ExpectedLOS-NLOS-AssistancePerTRP-r17 ::= SEQUENCE {

dl-PRS-ID-r17 INTEGER (0..255),

nr-PhysCellID-r17 NR-PhysCellID-r16 OPTIONAL, -- Need ON

nr-CellGlobalID-r17 NCGI-r15 OPTIONAL, -- Need ON

nr-ARFCN-r17 ARFCN-ValueNR-r15 OPTIONAL, -- Need ON

nr-los-nlos-indicator-r17 CHOICE {

perTrp-r17 LOS-NLOS-Indicator-r17,

perResource-r17 SEQUENCE (SIZE (1..nrMaxSetsPerTrpPerFreqLayer-r16)) OF

NR-DL-PRS-ExpectedLOS-NLOS-AssistancePerResource-r17 },

...

}

NR-DL-PRS-ExpectedLOS-NLOS-AssistancePerResource-r17 ::=

SEQUENCE (SIZE (1..nrMaxResourcesPerSet-r16)) OF

LOS-NLOS-Indicator-r17

-- ASN1STOP

|  |
| --- |
| *NR-DL-PRS-ExpectedLOS-NLOS-Assistance* field descriptions |
| ***dl-PRS-ID***  This field specifies the DL-PRS ID of the TRP for which the LOS/NLOS Information is provided. |
| ***nr-PhysCellID***  This field specifies the physical Cell-ID of the TRP for which the LOS/NLOS Information is provided, as defined in TS 38.331 [35]. |
| ***nr-CellGlobalID***  This field specifies the NCGI, the globally unique identity of a cell in NR, of the TRP for which the LOS/NLOS Information is provided, as defined in TS 38.331 [35]. |
| ***nr-ARFCN***  This field specifies the NR-ARFCN of the TRP's CD-SSB (as defined in TS 38.300 [47]) corresponding to *nr-PhysCellID*. |
| ***nr-los-nlos-indicator***  This field provides the expected likelihood of a LOS propagation path from a TRP to the target device (choice *perTrp*) or for all DL-PRS Resources of the TRP (choice *perResource*). |

#### *– NR-DL-PRS-Info*

The IE *NR-DL-PRS-Info* defines downlink PRS configuration.

-- ASN1START

NR-DL-PRS-Info-r16 ::= SEQUENCE {

nr-DL-PRS-ResourceSetList-r16 SEQUENCE (SIZE (1..nrMaxSetsPerTrpPerFreqLayer-r16)) OF

NR-DL-PRS-ResourceSet-r16,

...

}

NR-DL-PRS-ResourceSet-r16 ::= SEQUENCE {

nr-DL-PRS-ResourceSetID-r16 NR-DL-PRS-ResourceSetID-r16,

dl-PRS-Periodicity-and-ResourceSetSlotOffset-r16

NR-DL-PRS-Periodicity-and-ResourceSetSlotOffset-r16,

dl-PRS-ResourceRepetitionFactor-r16 ENUMERATED {n2, n4, n6, n8, n16, n32, ...}

OPTIONAL, -- Need OP

dl-PRS-ResourceTimeGap-r16 ENUMERATED {s1, s2, s4, s8, s16, s32, ...}

OPTIONAL, -- Cond Rep

dl-PRS-NumSymbols-r16 ENUMERATED {n2, n4, n6, n12, ..., n1-v1800 },

dl-PRS-MutingOption1-r16 DL-PRS-MutingOption1-r16 OPTIONAL, -- Need OP

dl-PRS-MutingOption2-r16 DL-PRS-MutingOption2-r16 OPTIONAL, -- Need OP

dl-PRS-ResourcePower-r16 INTEGER (-60..50),

dl-PRS-ResourceList-r16 SEQUENCE (SIZE (1..nrMaxResourcesPerSet-r16)) OF

NR-DL-PRS-Resource-r16,

...

}

DL-PRS-MutingOption1-r16 ::= SEQUENCE {

dl-prs-MutingBitRepetitionFactor-r16

ENUMERATED { n1, n2, n4, n8, ... } OPTIONAL, -- Need OP

nr-option1-muting-r16 NR-MutingPattern-r16,

...

}

DL-PRS-MutingOption2-r16 ::= SEQUENCE {

nr-option2-muting-r16 NR-MutingPattern-r16,

...

}

NR-MutingPattern-r16 ::= CHOICE {

po2-r16 BIT STRING (SIZE(2)),

po4-r16 BIT STRING (SIZE(4)),

po6-r16 BIT STRING (SIZE(6)),

po8-r16 BIT STRING (SIZE(8)),

po16-r16 BIT STRING (SIZE(16)),

po32-r16 BIT STRING (SIZE(32)),

...

}

NR-DL-PRS-Resource-r16 ::= SEQUENCE {

nr-DL-PRS-ResourceID-r16 NR-DL-PRS-ResourceID-r16,

dl-PRS-SequenceID-r16 INTEGER (0.. 4095),

dl-PRS-CombSizeN-AndReOffset-r16 CHOICE {

n2-r16 INTEGER (0..1),

n4-r16 INTEGER (0..3),

n6-r16 INTEGER (0..5),

n12-r16 INTEGER (0..11),

...

},

dl-PRS-ResourceSlotOffset-r16 INTEGER (0..nrMaxResourceOffsetValue-1-r16),

dl-PRS-ResourceSymbolOffset-r16 INTEGER (0..12),

dl-PRS-QCL-Info-r16 DL-PRS-QCL-Info-r16 OPTIONAL, --Need ON

...,

[[

dl-PRS-ResourcePrioritySubset-r17 DL-PRS-ResourcePrioritySubset-r17 OPTIONAL -- Need ON

]],

[[

dl-PRS-ResourceSymbolOffset-v1800 INTEGER (13) OPTIONAL -- Need OR

]]

}

DL-PRS-QCL-Info-r16 ::= CHOICE {

ssb-r16 SEQUENCE {

pci-r16 NR-PhysCellID-r16,

ssb-Index-r16 INTEGER (0..63),

rs-Type-r16 ENUMERATED {typeC, typeD, typeC-plus-typeD}

},

dl-PRS-r16 SEQUENCE {

qcl-DL-PRS-ResourceID-r16 NR-DL-PRS-ResourceID-r16,

qcl-DL-PRS-ResourceSetID-r16 NR-DL-PRS-ResourceSetID-r16

}

}

NR-DL-PRS-Periodicity-and-ResourceSetSlotOffset-r16 ::= CHOICE {

scs15-r16 CHOICE {

n4-r16 INTEGER (0..3),

n5-r16 INTEGER (0..4),

n8-r16 INTEGER (0..7),

n10-r16 INTEGER (0..9),

n16-r16 INTEGER (0..15),

n20-r16 INTEGER (0..19),

n32-r16 INTEGER (0..31),

n40-r16 INTEGER (0..39),

n64-r16 INTEGER (0..63),

n80-r16 INTEGER (0..79),

n160-r16 INTEGER (0..159),

n320-r16 INTEGER (0..319),

n640-r16 INTEGER (0..639),

n1280-r16 INTEGER (0..1279),

n2560-r16 INTEGER (0..2559),

n5120-r16 INTEGER (0..5119),

n10240-r16 INTEGER (0..10239),

...

},

scs30-r16 CHOICE {

n8-r16 INTEGER (0..7),

n10-r16 INTEGER (0..9),

n16-r16 INTEGER (0..15),

n20-r16 INTEGER (0..19),

n32-r16 INTEGER (0..31),

n40-r16 INTEGER (0..39),

n64-r16 INTEGER (0..63),

n80-r16 INTEGER (0..79),

n128-r16 INTEGER (0..127),

n160-r16 INTEGER (0..159),

n320-r16 INTEGER (0..319),

n640-r16 INTEGER (0..639),

n1280-r16 INTEGER (0..1279),

n2560-r16 INTEGER (0..2559),

n5120-r16 INTEGER (0..5119),

n10240-r16 INTEGER (0..10239),

n20480-r16 INTEGER (0..20479),

...

},

scs60-r16 CHOICE {

n16-r16 INTEGER (0..15),

n20-r16 INTEGER (0..19),

n32-r16 INTEGER (0..31),

n40-r16 INTEGER (0..39),

n64-r16 INTEGER (0..63),

n80-r16 INTEGER (0..79),

n128-r16 INTEGER (0..127),

n160-r16 INTEGER (0..159),

n256-r16 INTEGER (0..255),

n320-r16 INTEGER (0..319),

n640-r16 INTEGER (0..639),

n1280-r16 INTEGER (0..1279),

n2560-r16 INTEGER (0..2559),

n5120-r16 INTEGER (0..5119),

n10240-r16 INTEGER (0..10239),

n20480-r16 INTEGER (0..20479),

n40960-r16 INTEGER (0..40959),

...

},

scs120-r16 CHOICE {

n32-r16 INTEGER (0..31),

n40-r16 INTEGER (0..39),

n64-r16 INTEGER (0..63),

n80-r16 INTEGER (0..79),

n128-r16 INTEGER (0..127),

n160-r16 INTEGER (0..159),

n256-r16 INTEGER (0..255),

n320-r16 INTEGER (0..319),

n512-r16 INTEGER (0..511),

n640-r16 INTEGER (0..639),

n1280-r16 INTEGER (0..1279),

n2560-r16 INTEGER (0..2559),

n5120-r16 INTEGER (0..5119),

n10240-r16 INTEGER (0..10239),

n20480-r16 INTEGER (0..20479),

n40960-r16 INTEGER (0..40959),

n81920-r16 INTEGER (0..81919),

...

},

...

}

DL-PRS-ResourcePrioritySubset-r17 ::= SEQUENCE (SIZE (1..maxNumPrioResources-r17)) OF

NR-DL-PRSResourcePriorityItem-r17

NR-DL-PRSResourcePriorityItem-r17 ::= SEQUENCE {

nr-DL-PRS-PrioResourceSetID-r17 NR-DL-PRS-ResourceSetID-r16 OPTIONAL, -- Cond NotSame

nr-DL-PRS-PrioResourceID-r17 NR-DL-PRS-ResourceID-r16,

...

}

-- ASN1STOP

| Conditional presence | Explanation |
| --- | --- |
| *Rep* | The field is mandatory present, if *dl-PRS-ResourceRepetitionFactor* is present. Otherwise it is not present. |
| *NotSame* | The field is optionally present, need OP. If the field is absent, the indicated *nr-DL-PRS-PrioResourceID* belongs to the same DL-PRS Resource Set as the *nr-DL-PRS-ResourceID*. |

|  |
| --- |
| *NR-DL-PRS-Info* field descriptions |
| ***nr-DL-PRS-ResourceSetID***  This field specifies the DL-PRS Resource Set ID, which is used to identify the DL-PRS Resource Set of the TRP across all the frequency layers. |
| ***dl-PRS-Periodicity-and-ResourceSetSlotOffset***  This field specifies the periodicity of DL-PRS allocation in slots configured per DL-PRS Resource Set and the slot offset with respect to SFN #0 slot #0 for a TRP where the DL-PRS Resource Set is configured (i.e. slot where the first DL-PRS Resource of DL-PRS Resource Set occurs). |
| ***dl-PRS-ResourceRepetitionFactor***  This field specifies how many times each DL-PRS Resource is repeated for a single instance of the DL-PRS Resource Set. It is applied to all resources of the DL-PRS Resource Set. Enumerated values *n2*, *n4*, *n6*, *n8*, *n16*, *n32* correspond to 2, 4, 6, 8, 16, 32 resource repetitions, respectively. If this field is absent, the value for *dl-PRS-ResourceRepetitionFactor* is 1 (i.e., no resource repetition). |
| ***dl-PRS-ResourceTimeGap***  This field specifies the offset in units of slots between two repeated instances of a DL-PRS Resource corresponding to the same DL-PRS Resource ID within a single instance of the DL-PRS Resource Set. The time duration spanned by one DL-PRS Resource Set containing repeated DL-PRS Resources should not exceed DL-PRS-Periodicity. |
| ***dl-PRS-NumSymbols***  This field specifies the number of symbols per DL-PRS Resource within a slot. |
| ***dl-PRS-MutingOption1***  This field specifies the DL-PRS muting configuration of the TRP for the Option-1 muting, as specified in TS 38.214 [45], and comprises the following sub-fields:  - ***dl-prs-MutingBitRepetitionFactor*** indicates the number of consecutive instances of the DL-PRS Resource Set corresponding to a single bit of the *nr-option1-muting* bit map. Enumerated values *n1*, *n2*, *n4*, *n8* correspond to 1, 2, 4, 8 consecutive instances, respectively. If this sub-field is absent, the value for *dl-prs-MutingBitRepetitionFactor* is *n1*.  - ***nr-option1-muting*** defines a bitmap of the time locations where the DL-PRS Resource is transmitted (value '1') or not (value '0') for a DL-PRS Resource Set, as specified in TS 38.214 [45].  If this field is absent, Option-1 muting is not in use for the TRP. |
| ***dl-PRS-MutingOption2***  This field specifies the DL-PRS muting configuration of the TRP for the Option-2 muting, as specified in TS 38.214 [45], and comprises the following sub-fields:  - ***nr-option2-muting*** defines a bitmap of the time locations where the DL-PRS Resource is transmitted (value '1') or not (value '0'). Each bit of the bitmap corresponds to a single repetition of the DL-PRS Resource within an instance of a DL-PRS Resource Set, as specified in TS 38.214 [45]. The size of this bitmap should be the same as the value for *dl-PRS-ResourceRepetitionFactor*.  If this field is absent, Option-2 muting is not in use for the TRP. |
| ***dl-PRS-ResourcePower***  This field specifies the average EPRE of the resources elements that carry the DL-PRS in dBm that is used for PRS transmission. The UE assumes constant EPRE is used for all REs of a given DL-PRS Resource. |
| ***dl-PRS-SequenceID***  This field specifies the sequence Id used to initialize cinit value used in pseudo random generator TS 38.211 [41], clause 5.2.1 for generation of DL-PRS sequence for transmission on a given DL-PRS Resource. |
| ***dl-PRS-CombSizeN-AndReOffset***  This field specifies the Resource Element spacing in each symbol of the DL-PRS Resource and the Resource Element (RE) offset in the frequency domain for the first symbol in a DL-PRS Resource. All DL-PRS Resource Sets belonging to the same Positioning Frequency Layer have the same value of comb size. The relative RE offsets of following symbols are defined relative to the RE Offset in the frequency domain of the first symbol in the DL-PRS Resource according to TS 38.211 [41]. The comb size configuration should be aligned with the comb size configuration for the frequency layer. |
| ***dl-PRS-ResourceSlotOffset***  This field specifies the starting slot of the DL-PRS Resource with respect to the corresponding DL-PRS-Resource Set Slot Offset**.** |
| ***dl-PRS-ResourceSymbolOffset***  This field specifies the starting symbol of the DL-PRS Resource within a slot determined by *dl-PRS-ResourceSlotOffset*. If *dl-PRS-ResourceSymbolOffset-v1800* is present, the target device shall ignore *dl-PRS-ResourceSymbolOffset-r16*. |
| ***dl-PRS-QCL-Info***  This field specifies the QCL indication for a DL-PRS Resource with another DL reference signal from serving or neighbouring cell as defined in TS 38.214 [45], clause 5.1.6.5 and comprises the following subfields:  - ***ssb*** indicates the SSB information for QCL source and comprises the following sub-fields:  - ***pci*** specifies the physical cell ID of the cell with the SSB that is configured as the source reference signal for the DL-PRS Resource. The UE obtains the SSB configuration for the SSB configured as source reference signal for the DL-PRS Resource by selecting an SSB configuration from *nr-SSB-Config* with a matching physical cell identity.  - ***ssb-Index*** indicates the index for the SSB configured as the source reference signal for the DL-PRS Resource.  - ***rs-Type*** indicates the QCL type as defined in TS 38.214 [45], clause 5.1.6.5.  - ***dl-PRS*** indicates the DL-PRS source reference signal information for QCL typeD as defined in TS 38.214 [45], clause 5.1.6.5 and comprises the followings sub-fields:  - ***qcl-DL-PRS-ResourceID*** specifies DL-PRS Resource ID of the DL-PRS Resource used as the source reference signal.  - ***qcl-DL-PRS-ResourceSetID*** indicates the DL-PRS Resource Set ID of the DL-PRS Resource Set used as the source reference signal. |
| ***dl-PRS-ResourcePrioritySubset***  This field provides a subset of DL-PRS Resources, which is associated with *nr-DL-PRS-ResourceID* for the purpose of prioritization of DL-AoD reporting, as specified in TS 38.214 [45].  NOTE: This field is only applicable to DL-AoD positioning method and should be ignored for DL-TDOA, Multi-RTT, and NR AI/ML positioning. |

Editor's Note: It is FFS whether DL-PRS assistance data are needed for AI/ML positioning.

#### *– NR-DL-PRS-MeasurementTimeWindowsConfig*

The IE *NR-DL-PRS-MeasurementTimeWindowsConfig* provides a set of indicated time window(s) which is configured for the target device to perform measurements on indicated DL-PRS Resource Set(s) occurring within indicated time window(s).

-- ASN1START

NR-DL-PRS-MeasurementTimeWindowsConfig-r18 ::=

SEQUENCE (SIZE(1..2)) OF

NR-DL-PRS-MeasurementTimeWindowsConfigElement-r18

NR-DL-PRS-MeasurementTimeWindowsConfigElement-r18 ::= SEQUENCE {

nr-StartSFN-TimeWindow-r18 INTEGER (0..1023),

nr-PeriodicOrOneShotTimeWindow-r18 CHOICE {

nr-PeriodicityAndSlotOffsetTimeWindow-r18

NR-DL-PRS-Periodicity-and-ResourceSetSlotOffset-r16,

nr-OneShotSlotOffsetTimeWindow-r18 CHOICE {

scs15-r18 INTEGER (0..10239),

scs30-r18 INTEGER (0..20479),

scs60-r18 INTEGER (0..40959),

scs120-r18 INTEGER (0..81919)

}

} OPTIONAL, -- Need ON

nr-SymbolOffsetTimeWindow-r18 INTEGER (0..13) OPTIONAL, -- Need ON

nr-DurationTimeWindow-r18 ENUMERATED { n1, n2, n4, n6, n8, n12, n16, ... },

nr-SelectedDL-PRS-FrequencyLayerIndex-r18 INTEGER (0..nrMaxFreqLayers-1-r16)

OPTIONAL, -- Need ON

nr-SelectedDL-PRS-IndexListPerFreq-r18

SEQUENCE (SIZE (1..nrMaxTRPsPerFreq-r16)) OF

NR-SelectedDL-PRS-IndexPerTRP-r18 OPTIONAL, -- Need OP

nr-MeasurementsToPerformInTimeWindow-r18 BIT STRING { rstd (0),

ueRxTx (1),

rsrp (2),

rsrpp (3),

rscp (4),

rscpd (5)

} (SIZE(1..16)) OPTIONAL, -- Need ON

...

}

NR-SelectedDL-PRS-IndexPerTRP-r18 ::= SEQUENCE {

nr-SelectedTRP-Index-r18 INTEGER (0..nrMaxTRPsPerFreq-1-r16),

dl-SelectedPRS-ResourceSetIndexList-r18 SEQUENCE (SIZE (1..nrMaxSetsPerTrpPerFreqLayer-r16)) OF

INTEGER (0..nrMaxSetsPerTrpPerFreqLayer-1-r16) OPTIONAL, --Need OP

...

}

-- ASN1STOP

|  |
| --- |
| *NR-DL-PRS-MeasurementTimeWindowsConfig* field descriptions |
| ***nr-StartSFN-TimeWindow***  This field specifies the start of the time window in system frame number. |
| ***nr-PeriodicOrOneShotTimeWindow***  A one-shot field specifies the slot offset of the periodic or one-shot time window with respect to the SFN in IE *nr-StartSFN-TimeWindow* slot #0 for the TRP where the DL-PRS Resource Set is configured, and the periodicity of the periodic time window in slots configured per DL-PRS Resource Set. |
| ***nr-SymbolOffsetTimeWindow***  This field specifies the symbol offset with respect to the slot offset in *nr-PeriodicOrOneShotTimeWindow*. |
| ***nr-DurationTimeWindow***  This field specifies the desired duration of a time window for the indicated DL-PRS Resource Set in unit of slots. Enumerated value 'n1' corresponds to 1 slot, n2 to 2 slots, n4 to 4 slots and so on. |
| ***nr-SelectedDL-PRS-FrequencyLayerIndex***  This field indicates the frequency layer provided in IE *NR-DL-PRS-AssistanceData*. Value 0 corresponds to the first frequency layer provided in *nr-DL-PRS-AssistanceDataList* in IE *NR-DL-PRS-AssistanceData*, value 1 to the second frequency layer in *nr-DL-PRS-AssistanceDataList*, and so on. |
| ***nr-SelectedDL-PRS-IndexListPerFreq***  This field provides the list of addressed TRPs of the selected frequency layer. If this field is absent, all DL-PRS Resources of all TRPs of the indicated frequency layer are addressed. The number of the indicated DL-PRS Resource Set(s) for all the selected TRPs in this list is the same. |
| ***nr-SelectedTRP-Index***  This field indicates the addressed TRP of the selected frequency layer. Value 0 corresponds to the first entry in *nr-DL-PRS-AssistanceDataPerFreq* provided in IE *NR-DL-PRS-AssistanceData*, value 1 corresponds to the second entry in *nr-DL-PRS-AssistanceDataPerFreq*, and so on. |
| ***dl-SelectedPRS-ResourceSetIndexList***  This field provides the list of addressed DL-PRS Resource Sets of the selected TRPs of the selected frequency layer. If this field is absent, all DL-PRS Resource Sets and Resources of the indicated TRP are addressed. |
| ***nr-MeasurementsToPerformInTimeWindow***  This field indicates the measurements that UE shall perform in the configured time window. If multiple bits are set to 1, then UE shall perform multiple measurements in the same time window. |

#### *– NR-DL-PRS-ProcessingCapability*

The IE *NR-DL-PRS-ProcessingCapability* defines the common DL-PRS Processing capability. In the case of capabilities for multiple NR positioning methods are provided, the IE *NR-DL-PRS-ProcessingCapability* applies across the NR positioning methods and the target device shall indicate the same values for the capabilities in IEs *NR-DL-TDOA-ProvideCapabilities*, *NR-DL-AoD-ProvideCapabilities*, and *NR-Multi-RTT-ProvideCapabilities*.

Editor's Note: It is FFS whether the *NR-DL-PRS-ProcessingCapability* is also needed for AI/ML positioning.

The *PRS-ProcessingCapabilityPerBand* is defined for a single positioning frequency layer on a certain band (i.e., a target device supporting multiple positioning frequency layers is expected to process one frequency layer at a time).

-- ASN1START

NR-DL-PRS-ProcessingCapability-r16 ::= SEQUENCE {

prs-ProcessingCapabilityBandList-r16 SEQUENCE (SIZE (1..nrMaxBands-r16)) OF

PRS-ProcessingCapabilityPerBand-r16,

maxSupportedFreqLayers-r16 INTEGER (1..4),

simulLTE-NR-PRS-r16 ENUMERATED { supported } OPTIONAL,

...,

[[

dummy ENUMERATED { m1, m2, ... } OPTIONAL

]]

}

PRS-ProcessingCapabilityPerBand-r16 ::= SEQUENCE {

freqBandIndicatorNR-r16 FreqBandIndicatorNR-r16,

supportedBandwidthPRS-r16 CHOICE {

fr1 ENUMERATED {mhz5, mhz10, mhz20, mhz40,

mhz50, mhz80, mhz100},

fr2 ENUMERATED {mhz50, mhz100, mhz200, mhz400},

...

},

dl-PRS-BufferType-r16 ENUMERATED {type1, type2, ...},

durationOfPRS-Processing-r16 SEQUENCE {

durationOfPRS-ProcessingSymbols-r16 ENUMERATED {nDot125, nDot25, nDot5, n1,

n2, n4, n6, n8, n12, n16, n20, n25,

n30, n32, n35, n40, n45, n50},

durationOfPRS-ProcessingSymbolsInEveryTms-r16

ENUMERATED {n8, n16, n20, n30, n40, n80,

n160,n320, n640, n1280},

...

},

maxNumOfDL-PRS-ResProcessedPerSlot-r16 SEQUENCE {

scs15-r16 ENUMERATED {n1, n2, n4, n8, n16, n24, n32,

n48, n64} OPTIONAL,

scs30-r16 ENUMERATED {n1, n2, n4, n8, n16, n24, n32,

n48, n64} OPTIONAL,

scs60-r16 ENUMERATED {n1, n2, n4, n8, n16, n24, n32,

n48, n64} OPTIONAL,

scs120-r16 ENUMERATED {n1, n2, n4, n8, n16, n24, n32,

n48, n64} OPTIONAL,

...,

[[

scs15-v1690 ENUMERATED {n6, n12} OPTIONAL,

scs30-v1690 ENUMERATED {n6, n12} OPTIONAL,

scs60-v1690 ENUMERATED {n6, n12} OPTIONAL,

scs120-v1690 ENUMERATED {n6, n12} OPTIONAL

]]

},

...,

[[

supportedDL-PRS-ProcessingSamples-RRC-CONNECTED-r17 ENUMERATED { supported } OPTIONAL,

prs-ProcessingWindowType1A-r17 ENUMERATED { option1, option2, option3} OPTIONAL,

prs-ProcessingWindowType1B-r17 ENUMERATED { option1, option2, option3} OPTIONAL,

prs-ProcessingWindowType2-r17 ENUMERATED { option1, option2, option3} OPTIONAL,

prs-ProcessingCapabilityOutsideMGinPPW-r17

SEQUENCE (SIZE(1..3)) OF

PRS-ProcessingCapabilityOutsideMGinPPWperType-r17

OPTIONAL,

dl-PRS-BufferType-RRC-Inactive-r17 ENUMERATED { type1, type2, ... } OPTIONAL,

durationOfPRS-Processing-RRC-Inactive-r17 SEQUENCE {

durationOfPRS-ProcessingSymbols-r17 ENUMERATED {nDot125, nDot25, nDot5, n1,

n2, n4, n6, n8, n12, n16, n20, n25,

n30, n32, n35, n40, n45, n50},

durationOfPRS-ProcessingSymbolsInEveryTms-r17

ENUMERATED {n8, n16, n20, n30, n40, n80,

n160,n320, n640, n1280},

...

} OPTIONAL,

maxNumOfDL-PRS-ResProcessedPerSlot-RRC-Inactive-r17 SEQUENCE {

scs15-r17 ENUMERATED {n1, n2, n4, n6, n8, n12, n16, n24,

n32, n48, n64} OPTIONAL,

scs30-r17 ENUMERATED {n1, n2, n4, n6, n8, n12, n16, n24,

n32, n48, n64} OPTIONAL,

scs60-r17 ENUMERATED {n1, n2, n4, n6, n8, n12, n16, n24,

n32, n48, n64} OPTIONAL,

scs120-r17 ENUMERATED {n1, n2, n4, n6, n8, n12, n16, n24,

n32, n48, n64} OPTIONAL,

...

} OPTIONAL,

supportedLowerRxBeamSweepingFactor-FR2-r17 ENUMERATED { n1, n2, n4, n6 } OPTIONAL

]],

[[

supportedDL-PRS-ProcessingSamples-RRC-Inactive-r17 ENUMERATED { supported } OPTIONAL

]],

[[

prs-MeasurementWithoutMG-r17 ENUMERATED {cp, symbolDot25, symbolDot5,

slotDot5} OPTIONAL

]],

[[

maxNumOfOneSymbolPRS-ResProcessedPerSlot-RRC-Inactive-r18 SEQUENCE {

scs15-r18 ENUMERATED {n1, n2, n4, n6, n8, n12, n16, n24,

n32, n48, n64} OPTIONAL,

scs30-r18 ENUMERATED {n1, n2, n4, n6, n8, n12, n16, n24,

n32, n48, n64} OPTIONAL,

scs60-r18 ENUMERATED {n1, n2, n4, n6, n8, n12, n16, n24,

n32, n48, n64} OPTIONAL,

scs120-r18 ENUMERATED {n1, n2, n4, n6, n8, n12, n16, n24,

n32, n48, n64} OPTIONAL,

...

} OPTIONAL,

maxNumOfOneSymbolPRS-ResProcessedPerSlot-RRC-Connected-r18 SEQUENCE {

scs15-r18 ENUMERATED {n1, n2, n4, n6, n8, n12, n16, n24,

n32, n48, n64} OPTIONAL,

scs30-r18 ENUMERATED {n1, n2, n4, n6, n8, n12, n16, n24,

n32, n48, n64} OPTIONAL,

scs60-r18 ENUMERATED {n1, n2, n4, n6, n8, n12, n16, n24,

n32, n48, n64} OPTIONAL,

scs120-r18 ENUMERATED {n1, n2, n4, n6, n8, n12, n16, n24,

n32, n48, n64} OPTIONAL,

...

} OPTIONAL,

ppw-maxNumOfOneSymbolPRS-ResProcessedPerSlot-r18 SEQUENCE {

scs15-r18 ENUMERATED {n1, n2, n4, n6, n8, n12, n16, n24,

n32, n48, n64} OPTIONAL,

scs30-r18 ENUMERATED {n1, n2, n4, n6, n8, n12, n16, n24,

n32, n48, n64} OPTIONAL,

scs60-r18 ENUMERATED {n1, n2, n4, n6, n8, n12, n16, n24,

n32, n48, n64} OPTIONAL,

scs120-r18 ENUMERATED {n1, n2, n4, n6, n8, n12, n16, n24,

n32, n48, n64} OPTIONAL,

...

} OPTIONAL,

prs-BWA-TwoContiguousIntrabandInMG-RRC-Connected-r18

PRS-BWA-TwoContiguousIntrabandInMG-r18 OPTIONAL,

prs-BWA-ThreeContiguousIntrabandInMG-RRC-Connected-r18

PRS-BWA-ThreeContiguousIntrabandInMG-r18 OPTIONAL,

prs-BWA-TwoContiguousIntraband-RRC-IdleAndInactive-r18

PRS-BWA-TwoContiguousIntrabandInMG-r18 OPTIONAL,

prs-BWA-ThreeContiguousIntraband-RRC-IdleAndInactive-r18

PRS-BWA-ThreeContiguousIntrabandInMG-r18 OPTIONAL,

reducedNumOfSampleInMeasurementWithPRS-BWA-RRC-Connected-r18 ENUMERATED { supported }

OPTIONAL,

reducedNumOfSampleInMeasurementWithPRS-BWA-RRC-IdleAndInactive-r18

ENUMERATED { supported } OPTIONAL,

dl-PRS-MeasurementWithRxFH-RRC-Inactive-r18 ENUMERATED { supported } OPTIONAL,

dl-PRS-MeasurementWithRxFH-RRC-Idle-r18 ENUMERATED { supported } OPTIONAL,

reducedNumOfSampleForMeasurementWithFH-RRC-Connected-r18 ENUMERATED { supported }

OPTIONAL,

reducedNumOfSampleForMeasurementWithFH-RRC-IdleAndInactive-r18 ENUMERATED { supported }

OPTIONAL,

supportOfPRS-BWA-WithTwoPFL-Combination-r18 ENUMERATED { supported } OPTIONAL,

dl-PRS-MeasurementWithRxFH-RRC-Connected-r18 DL-PRS-MeasurementWithRxFH-RRC-Connected-r18 OPTIONAL

]]

}

PRS-ProcessingCapabilityOutsideMGinPPWperType-r17 ::= SEQUENCE {

prsProcessingType-r17 ENUMERATED { type1A, type1B, type2 },

ppw-dl-PRS-BufferType-r17 ENUMERATED { type1, type2, ... },

ppw-durationOfPRS-Processing1-r17 SEQUENCE {

ppw-durationOfPRS-ProcessingSymbolsN-r17

ENUMERATED { msDot125, msDot25, msDot5, ms1, ms2, ms4,

ms6, ms8, ms12, ms16, ms20, ms25, ms30, ms32, ms35,

ms40, ms45, ms50 },

ppw-durationOfPRS-ProcessingSymbolsT-r17

ENUMERATED { ms1, ms2, ms4, ms8, ms16, ms20, ms30, ms40, ms80,

ms160, ms320, ms640, ms1280 }

} OPTIONAL,

ppw-durationOfPRS-Processing2-r17 SEQUENCE {

ppw-durationOfPRS-ProcessingSymbolsN2-r17

ENUMERATED { msDot125, msDot25, msDot5, ms1, ms2, ms3, ms4, ms5,

ms6, ms8, ms12 },

ppw-durationOfPRS-ProcessingSymbolsT2-r17

ENUMERATED { ms4, ms5, ms6, ms8 }

} OPTIONAL,

ppw-maxNumOfDL-PRS-ResProcessedPerSlot-r17 SEQUENCE {

scs15-r17 ENUMERATED {n1, n2, n4, n6, n8, n12,

n16, n24, n32, n48, n64 }

OPTIONAL,

scs30-r17 ENUMERATED {n1, n2, n4, n6, n8, n12,

n16, n24, n32, n48, n64 }

OPTIONAL,

scs60-r17 ENUMERATED {n1, n2, n4, n6, n8, n12,

n16, n24, n32, n48, n64 }

OPTIONAL,

scs120-r17 ENUMERATED {n1, n2, n4, n6, n8, n12,

n16, n24, n32, n48, n64 }

OPTIONAL,

...

},

...,

[[

ppw-maxNumOfDL-Bandwidth-r17 CHOICE {

fr1 ENUMERATED {mhz5, mhz10, mhz20, mhz40,

mhz50, mhz80, mhz100},

fr2 ENUMERATED {mhz50, mhz100, mhz200, mhz400}

} OPTIONAL

]]

}

PRS-BWA-TwoContiguousIntrabandInMG-r18 ::= SEQUENCE {

maximumOfTwoAggregatedDL-PRS-Bandwidth-FR1-r18 ENUMERATED {mhz10, mhz20, mhz40, mhz50,

mhz80, mhz100, mhz160, mhz200}

OPTIONAL,

maximumOfTwoAggregatedDL-PRS-Bandwidth-FR2-r18 ENUMERATED {mhz100, mhz200, mhz400, mhz800}

OPTIONAL,

maximumOfDL-PRS-BandwidthPerPFL-FR1-r18 ENUMERATED {mhz5, mhz10, mhz20, mhz40,

mhz50, mhz80, mhz100} OPTIONAL,

maximumOfDL-PRS-BandwidthPerPFL-FR2-r18 ENUMERATED {mhz50, mhz100, mhz200, mhz400}

OPTIONAL,

dl-PRS-BufferTypeOfBWA-r18 ENUMERATED {type1, type2},

prs-durationOfTwoPRS-BWA-Processing-r18 SEQUENCE {

prs-durationOfTwoPRS-BWA-ProcessingSymbolsN-r18

ENUMERATED {msDot125, msDot25, msDot5, ms1, ms2, ms4, ms6, ms8, ms12,

ms16, ms20, ms25, ms30, ms32, ms35, ms40, ms45, ms50},

prs-durationOfTwoPRS-BWA-ProcessingSymbolsT-r18

ENUMERATED {ms8, ms16, ms20, ms30, ms40, ms80, ms160, ms320, ms640, ms1280}

} OPTIONAL,

maxNumOfAggregatedDL-PRS-ResourcePerSlot-FR1-r18 SEQUENCE {

scs15-r18 ENUMERATED {n1, n2, n4, n6, n8, n12,

n16, n24, n32, n48, n64 } OPTIONAL,

scs30-r18 ENUMERATED {n1, n2, n4, n6, n8, n12,

n16, n24, n32, n48, n64 } OPTIONAL,

scs60-r18 ENUMERATED {n1, n2, n4, n6, n8, n12,

n16, n24, n32, n48, n64 } OPTIONAL

},

maxNumOfAggregatedDL-PRS-ResourcePerSlot-FR2-r18 SEQUENCE {

scs60-r18 ENUMERATED {n1, n2, n4, n6, n8, n12,

n16, n24, n32, n48, n64 } OPTIONAL,

scs120-r18 ENUMERATED {n1, n2, n4, n6, n8, n12,

n16, n24, n32, n48, n64 } OPTIONAL

}

}

PRS-BWA-ThreeContiguousIntrabandInMG-r18 ::= SEQUENCE {

maximumOfThreeAggregatedDL-PRS-Bandwidth-FR1-r18

ENUMERATED {mhz15, mhz20, mhz30, mhz40, mhz50, mhz60, mhz80, mhz100, mhz120,

mhz140, mhz150, mhz180, mhz200, mhz240, mhz300} OPTIONAL,

maximumOfThreeAggregatedDL-PRS-Bandwidth-FR2-r18

ENUMERATED {mhz150, mhz200, mhz300, mhz400, mhz600, mhz800, mhz1000,

mhz1200} OPTIONAL,

maximumOfDL-PRS-BandwidthPerPFL-FR1-r18

ENUMERATED {mhz5, mhz10, mhz20, mhz40, mhz50, mhz80, mhz100} OPTIONAL,

maximumOfDL-PRS-BandwidthPerPFL-FR2-r18

ENUMERATED {mhz50, mhz100, mhz200, mhz400} OPTIONAL,

dl-PRS-BufferTypeOfBWA-r18 ENUMERATED {type1, type2},

prs-durationOfThreePRS-BWA-Processing-r18 SEQUENCE {

prs-durationOfThreePRS-BWA-ProcessingSymbolsN-r18

ENUMERATED {msDot125, msDot25, msDot5, ms1, ms2, ms4, ms6, ms8, ms12,

ms16, ms20, ms25, ms30, ms32, ms35, ms40, ms45, ms50},

prs-durationOfThreePRS-BWA-ProcessingSymbolsT-r18

ENUMERATED {ms8, ms16, ms20, ms30, ms40, ms80, ms160,

ms320, ms640, ms1280}

} OPTIONAL,

maxNumOfAggregatedDL-PRS-ResourcePerSlot-FR1-r18 SEQUENCE {

scs15-r18 ENUMERATED {n1, n2, n4, n6, n8, n12,

n16, n24, n32, n48, n64 } OPTIONAL,

scs30-r18 ENUMERATED {n1, n2, n4, n6, n8, n12,

n16, n24, n32, n48, n64 } OPTIONAL,

scs60-r18 ENUMERATED {n1, n2, n4, n6, n8, n12,

n16, n24, n32, n48, n64 } OPTIONAL

},

maxNumOfAggregatedDL-PRS-ResourcePerSlot-FR2-r18 SEQUENCE {

scs60-r18 ENUMERATED {n1, n2, n4, n6, n8, n12,

n16, n24, n32, n48, n64 } OPTIONAL,

scs120-r18 ENUMERATED {n1, n2, n4, n6, n8, n12,

n16, n24, n32, n48, n64 } OPTIONAL

}

}

DL-PRS-MeasurementWithRxFH-RRC-Connected-r18 ::=SEQUENCE {

maximumPRS-BandwidthAcrossAllHopsFR1-r18 ENUMERATED {mhz40, mhz50, mhz80, mhz100}

OPTIONAL,

maximumPRS-BandwidthAcrossAllHopsFR2-r18 ENUMERATED {mhz100, mhz200, mhz400} OPTIONAL,

maximumFH-Hops-r18 ENUMERATED {n2, n3, n4, n5, n6} OPTIONAL,

processingDuration-r18 SEQUENCE {

processingPRS-SymbolsDurationN3-r18 ENUMERATED {msDot125, msDot25, msDot5, ms1, ms2,

ms4, ms6, ms8, ms12,ms16, ms20, ms25,

ms30, ms32, ms35, ms40, ms45, ms50},

processingDurationT3-r18 ENUMERATED {ms8, ms16, ms20, ms30, ms40, ms80,

ms160, ms320, ms640, ms1280}

} OPTIONAL,

rf-RxRetuneTimeFR1-r18 ENUMERATED {n70,n140,n210} OPTIONAL,

rf-RxRetuneTimeFR2-r18 ENUMERATED {n35,n70,n140} OPTIONAL,

numOfOverlappingPRB-r18 ENUMERATED {n0,n1,n2,n4} OPTIONAL,

...

}

-- ASN1STOP

| *NR-DL-PRS-ProcessingCapability* field descriptions |
| --- |
| ***maxSupportedFreqLayers***  Indicates the maximum number of positioning frequency layers supported by UE. |
| ***simulLTE-NR-PRS***  Indicates whether the UE supports parallel processing of LTE PRS and NR DL-PRS. |
| ***dummy***  This field is not used in the specification. If received it shall be ignored by the receiver. |
| ***supportedBandwidthPRS***  Indicates the maximum number of DL-PRS bandwidth in MHz, which is supported and reported by UE. |
| ***dl-PRS-BufferType***  IndicatesDL-PRS buffering capability. Value *type1* indicates sub-slot/symbol level buffering and value *type2* indicates slot level buffering. |
| ***durationOfPRS-Processing***  Indicates the duration *N* of DL-PRS symbols in units of ms a UE can process every T ms assuming maximum DL-PRS bandwidth provided in *supportedBandwidthPRS* and comprises the following subfields:  - ***durationOfPRS-ProcessingSymbols***: This field specifies the values for *N*. Enumerated values indicate 0.125, 0.25, 0.5, 1, 2, 4, 6, 8, 12, 16, 20, 25, 30, 32, 35, 40, 45, 50 ms.  - ***durationOfPRS-ProcessingSymbolsInEveryTms***: This field specifies the values for *T*. Enumerated values indicate 8, 16, 20, 30, 40, 80, 160, 320, 640, 1280 ms.  See NOTE 9. |
| ***maxNumOfDL-PRS-ResProcessedPerSlot***  Indicates the maximum number of DL-PRS Resources that UE can process in a slot. SCS: 15 kHz, 30 kHz, 60 kHz are applicable for FR1 bands. SCS: 60 kHz, 120 kHz are applicable for FR2 bands. |
| ***supportedDL-PRS-ProcessingSamples-RRC-CONNECTED***  Indicates the UE capability for support of measurements based on measuring M=1 or M=2 (instances) of a DL-PRS Resource Set. The UE can include this field only if the UE supports *prs-ProcessingCapabilityBandList*. Otherwise, the UE does not include this field.  NOTE 1: This feature is supported for both UE-assisted and UE based positioning. |
| ***prs-ProcessingWindowType1A***  Indicates the supported DL-PRS processing types subject to the UE determining that DL-PRS to be higher priority for DL-PRS measurement outside MG and in a DL-PRS Processing Window.  Type 1A refers to the determination of prioritization between DL-PRS and other DL signals/channels in all OFDM symbols within the DL-PRS Processing Window. The DL signals/channels from all DL CCs (per UE) are affected across LTE and NR. Enumerated value indicates supported priority handing options of DL-PRS:  - *option1*: Support of "st1" and "st3" defined in clause 5.1.6.5 of TS 38.214 [45].  - *option2*: Support of "st1", "st2", and "st3" defined in clause 5.1.6.5 of TS 38.214 [45].  - *option3*: Support of "st1" only defined in clause 5.1.6.5 of TS 38.214 [45].  The UE can include this field only if the UE supports *prs-ProcessingCapabilityBandList*. Otherwise, the UE does not include this field.  NOTE 2: Within a DL-PRS processing window, UE measurement is inside the active DL BWP with DL-PRS having the same numerology as the active DL BWP.  NOTE 2a: When the UE determines higher priority for other DL signals/channels over the DL-PRS measurement/processing, the UE is not expected to measure/process DL-PRS. |
| ***prs-ProcessingWindowType1B***  Indicates the supported DL-PRS processing types subject to the UE determining that DL-PRS to be higher priority for DL-PRS measurement outside MG and in a DL-PRS Processing Window.  Type 1B refers to the determination of prioritization between DL-PRS and other DL signals/channels in all OFDM symbols within the DL-PRS processing window. The DL signals/channels from a certain band are affected. Enumerated value indicates supported priority handing options of DL-PRS (see *prs-ProcessingWindowType1A*).  The UE can include this field only if the UE supports prs-ProcessingCapabilityBandList. Otherwise, the UE does not include this field.  NOTE 3: Within a DL-PRS processing window, UE measurement is inside the active DL BWP with DL-PRS having the same numerology as the active DL BWP.  NOTE 3a: When the UE determines higher priority for other DL signals/channels over the DL-PRS measurement/processing, the UE is not expected to measure/process DL-PRS. |
| ***prs-ProcessingWindowType2***  Indicates the supported DL-PRS processing types subject to the UE determining that DL-PRS to be higher priority for DL-PRS measurement outside MG and in a DL-PRS Processing Window.  Type 2 refers to the determination of prioritization between DL-PRS and other DL signals/channels only in DL-PRS symbols within the DL-PRS processing window. Enumerated value indicates supported priority handing options of DL-PRS (see *prs-ProcessingWindowType1A*).  The UE can include this field only if the UE supports *prs-ProcessingCapabilityBandList*. Otherwise, the UE does not include this field.  NOTE 4: Within a DL-PRS processing window, UE measurement is inside the active DL BWP with DL-PRS having the same numerology as the active DL BWP.  NOTE 4a: When the UE determines higher priority for other DL signals/channels over the DL-PRS measurement/processing, the UE is not expected to measure/process DL-PRS. |
| ***prs-ProcessingCapabilityOutsideMGinPPW***  Indicates the DL-PRS Processing Capability outside MG of each of the supported PPW Type in the case the UE supports multiple PPW Types in a band and comprises the following subfields:  - ***prsProcessingType***: Indicates the DL-PRS Processing Window Type for which the *prs-ProcessingCapabilityOutsideMGinPPW* are provided.  - ***ppw-dl-PRS-BufferType***: Indicates DL-PRS buffering capability. Value '*type1'* indicates sub-slot/symbol level buffering and value '*type2'* indicates slot level buffering.  - ***ppw-durationOfPRS-Processing1***: Indicates the duration of DL-PRS symbols N in units of ms a UE can process every T ms assuming maximum DL-PRS bandwidth provided in *ppw-maxNumOfDL-Bandwidth* and comprises the following subfields:  - ***ppw-durationOfPRS-ProcessingSymbolsN***: This field specifies the values for *N*. Enumerated values indicate 0.125, 0.25, 0.5, 1, 2, 4, 6, 8, 12, 16, 20, 25, 30, 32, 35, 40, 45, 50 ms.  - ***ppw-durationOfPRS-ProcessingSymbolsT***: This field specifies the values for *T*. Enumerated values indicate 1, 2, 4, 8, 16, 20, 30, 40, 80, 160, 320, 640, 1280 ms.  - ***ppw-durationOfPRS-Processing2***: Indicates the duration of DL-PRS symbols N2 in units of ms a UE can process inT2 ms assuming maximum DL-PRS bandwidth provided in *ppw-maxNumOfDL-Bandwidth* and comprises the following subfields:  - ***ppw-durationOfPRS-ProcessingSymbolsN2***: This field specifies the values for *N2*. Enumerated values indicate 0.125, 0.25, 0.5, 1, 2, 3, 4, 5, 6, 8, 12 ms.  - ***ppw-durationOfPRS-ProcessingSymbolsT2***: This field specifies the values for *T2*. Enumerated values indicate 4, 5, 6, 8 ms.  - ***ppw-maxNumOfDL-PRS-ResProcessedPerSlot:*** Indicates the maximum number of DL-PRS resources that UE can process in a slot. SCS: 15 kHz, 30 kHz, 60 kHz are applicable for FR1 bands. SCS: 60 kHz, 120 kHz are applicable for FR2 bands.  - ***ppw-maxNumOfDL-Bandwidth:*** Indicates the maximum number of DL-PRS bandwidth in MHz, which is supported and reported by UE for DL-PRS measurement outside MG within the PPW.  The UE can include this field only if the UE supports one of *prs-ProcessingWindowType1A*, *prs-ProcessingWindowType1B* and *prs-ProcessingWindowType2*. Otherwise, the UE does not include this field.  NOTE 5: A UE that supports one of *prs-ProcessingWindowType1A*, *prs-ProcessingWindowType1B* or *prs-ProcessingWindowType2* shall always include the *prs-ProcessingCapabilityOutsideMGinPPW*.  NOTE 6: The (N, T) UE capability in *ppw-durationOfPRS-Processing1* is interpreted as in NOTE 9, and the UE is expected to receive the DL-PRS within the DL-PRS processing window but the processing of the received DL-PRS may be outside a DL-PRS processing window.  NOTE 7: The (N2, T2) UE capability in *ppw-durationOfPRS-Processing2* is interpreted such that the UE is capable of measuring up to N2 ms DL-PRS within a PPW and is capable of completing the DL-PRS processing within the PPW, e.g., if the time duration from the last symbol of the measured DL-PRS Resource(s) inside the PPW to the end of PPW is not smaller than T2 ms.  NOTE 8: A UE which supports *prs-ProcessingCapabilityOutsideMGinPPW* shall support either *ppw-durationOfPRS-Processing1* or *ppw-durationOfPRS-Processing2*, but not both for each supported type in a band. |
| ***dl-PRS-BufferType-RRC-Inactive***  IndicatesDL-PRS buffering capability in RRC\_INACTIVE state. Value '*type1'* indicates sub-slot/symbol level buffering and value '*type2'* indicates slot level buffering. |
| ***durationOfPRS-Processing-RRC-Inactive***  Indicates the duration *N* of DL-PRS symbols in units of ms a UE can process every *T* ms in RRC\_INACTIVE state assuming maximum DL-PRS bandwidth provided in *supportedBandwidthPRS* and comprises the following subfields:  - ***durationOfPRS-ProcessingSymbols***: This field specifies the values for *N*. Enumerated values indicate 0.125, 0.25, 0.5, 1, 2, 4, 6, 8, 12, 16, 20, 25, 30, 32, 35, 40, 45, 50 ms.  - ***durationOfPRS-ProcessingSymbolsInEveryTms***: This field specifies the values for *T*. Enumerated values indicate 8, 16, 20, 30, 40, 80, 160, 320, 640, 1280 ms.  See NOTE 9. |
| ***maxNumOfDL-PRS-ResProcessedPerSlot-RRC-Inactive***  Indicates the maximum number of DL-PRS Resources a UE can process in a slot in RRC\_INACTIVE state. SCS: 15 kHz, 30 kHz, 60 kHz are applicable for FR1 bands. SCS: 60 kHz, 120 kHz are applicable for FR2 bands. |
| ***supportedLowerRxBeamSweepingFactor-FR2***  Indicates support of the lower Rx beam sweeping factor than 8 for FR2. Enumerated value indicates the number of Rx beam sweeping factors supported. |
| ***supportedDL-PRS-ProcessingSamples-RRC-Inactive***  Indicates the UE capability for support of reduced number of samples for DL-PRS measurement in RRC\_INACTIVE state. The UE can include this field only if the UE supports *prs-ProcessingRRC-Inactive* defined in TS 38.331 [35]. Otherwise, the UE does not include this field. |
| ***maxNumOfOneSymbolPRS-ResProcessedPerSlot-RRC-Inactive***  Indicates the maximum number of single-symbol DL-PRS Resources that UE can process in a slot in RRC\_INACTIVE. SCS: 15 kHz, 30 kHz, 60 kHz are applicable for FR1 bands. SCS: 60 kHz, 120 kHz are applicable for FR2 bands. A UE which supports *maxNumOfOneSymbolPRS-ResProcessedPerSlot-RRC-Inactive* shall support single-symbol DL-PRS with the comb sizes from {2,4,6,12}.  The UE can include this field only if the UE supports one of *dl-PRS-BufferType-RRC-Inactive*, *durationOfPRS-Processing-RRC-Inactive*, and *maxNumOfDL-PRS-ResProcessedPerSlot-RRC-Inactive*. Otherwise, the UE does not include this field. |
| ***maxNumOfOneSymbolPRS-ResProcessedPerSlot-RRC-Connected***  Indicates the maximum number of single-symbol DL-PRS Resources that UE can process in a slot inside a measurement gap in RRC\_CONNECTED. SCS: 15 kHz, 30 kHz, 60 kHz are applicable for FR1 bands. SCS: 60 kHz, 120 kHz are applicable for FR2 bands. A UE which supports *maxNumOfOneSymbolPRS-ResProcessedPerSlot-RRC-Connected* shall support single-symbol DL-PRS with the comb sizes from {2,4,6,12}.  The UE can include this field only if the UE supports *prs-ProcessingCapabilityBandList*. Otherwise, the UE does not include this field. |
| ***ppw-maxNumOfOneSymbolPRS-ResProcessedPerSlot***  Indicates the maximum number of single-symbol DL-PRS Resources that UE can process in a slot outside a measurement gap in RRC\_CONNECTED. SCS: 15 kHz, 30 kHz, 60 kHz are applicable for FR1 bands. SCS: 60 kHz, 120 kHz are applicable for FR2 bands. A UE which supports *ppw-maxNumOfOneSymbolPRS-ResProcessedPerSlot* shall support single-symbol DL-PRS with the comb sizes from {2,4,6,12}.  The UE can include this field only if the UE supports *prs-ProcessingCapabilityOutsideMGinPPW*. Otherwise, the UE does not include this field. |
| ***prs-MeasurementWithoutMG***  Indicates the UE capability for support of Rx timing difference between the serving cell and non-serving cell for DL-PRS measurement within a PPW. Value '*cp*' indicates one CP length, value '*symbolDot25*' indicates 0.25 symbol length, value '*symbolDot5*' indicates 0.5 symbol length and value '*slotDot5*' indicates 0.5 slot length. The UE can include this field only if the UE supports one of *prs-ProcessingWindowType1A*, *prs-ProcessingWindowType1B* and *prs-ProcessingWindowType2*. Otherwise, the UE does not include this field. |
| ***prs-BWA-TwoContiguousIntrabandInMG-RRC-Connected***  Indicates the UE capability for support of DL-PRS processing capabilities for aggregated DL-PRS processing of 2 PFLs in intra-band contiguous within a MG for RRC\_CONNECTED state and and comprises the following subfields:  - ***maximumOfTwoAggregatedDL-PRS-Bandwidth-FR1***: Indicates the maximum aggregated DL-PRS bandwidth in MHz for FR1, which is supported and reported by UE.  - ***maximumOfTwoAggregatedDL-PRS-Bandwidth-FR2***: Indicates the maximum aggregated DL-PRS bandwidth in MHz for FR2, which is supported and reported by UE.  - ***maximumOfDL-PRS-BandwidthPerPFL-FR1***: Indicates the maximum DL-PRS bandwidth in MHz for FR1, per PFL.  - ***maximumOfDL-PRS-BandwidthPerPFL-FR2***: Indicates the maximum DL-PRS bandwidth in MHz for FR2, per PFL.  - ***dl-PRS-BufferTypeOfBWA***: Indicates the DL-PRS buffering capability.  - ***prs-durationOfTwoPRS-BWA-Processing***: Indicates the duration of DL-PRS symbols N in units of ms a UE can process every T ms assuming maximum aggregated DL-PRS bandwidth in MHz, which is supported and reported by UE.  - ***prs-durationOfTwoPRS-BWA-ProcessingSymbolsN***: This field specifies the values for N. Enumerated values indicate 0.125, 0.25, 0.5, 1, 2, 4, 6, 8, 12, 16, 20, 25, 30, 32, 35, 40, 45, 50 ms.  - ***prs-durationOfTwoPRS-BWA-ProcessingSymbolsT***: This field specifies the values for T. Enumerated values indicate 8, 16, 20, 30, 40, 80, 160, 320, 640, 1280, 2560 ms.  - ***maxNumOfAggregatedDL-PRS-ResourcePerSlot-FR1***: Indicates the Maximum number of aggregated DL-PRS Resources across aggregated PFLs that UE can process in a slot for FR1.  - ***maxNumOfAggregatedDL-PRS-ResourcePerSlot-FR2***: Indicates the Maximum number of aggregated DL-PRS Resources across aggregated PFLs that UE can process in a slot for FR2.  The UE can include this field only if the UE supports *supportedBandwidthPRS, dl-PRS-BufferType, durationOfPRS-Processing* and *maxNumOfDL-PRS-ResProcessedPerSlot*. Otherwise, the UE does not include this field.  NOTE 10: *dl-PRS-BufferTypeOfBWA* follows buffering capability type reported in *dl-PRS-BufferType.*  NOTE 11: The value N should be equal or smaller than the value N reported by *durationOfPRS-ProcessingSymbols*, or this value T should be equal or larger than the value T reported by *durationOfPRS-ProcessingSymbolsInEveryTms.*  NOTE 12: Each two linked DL-PRS Resources are counted as 1 resource.  NOTE 13: *maxNumOfAggregatedDL-PRS-ResourcePerSlot* should be equal or smaller than the value reported by *maxNumOfDL-PRS-ResProcessedPerSlot.*  NOTE 14: The above parameters are reported assuming a configured measurement gap and a maximum ratio of measurement gap length (MGL)/measurement gap repetition period (MGRP) of no more than 30%. |
| ***prs-BWA-ThreeContiguousIntrabandInMG-RRC-Connected***  Indicates the UE capability for support of DL-PRS processing capabilities for aggregated DL-PRS processing of 3 PFLs in intra-band contiguous within a MG for RRC\_CONNECTED state and comprises the following subfields:  **- *maximumOfThreeAggregatedDL-PRS-Bandwidth-FR1***: Indicates the maximum aggregated DL-PRS bandwidth in MHz of for FR1, which is supported and reported by UE.  **- *maximumOfThreeAggregatedDL-PRS-Bandwidth-FR2***: Indicates the maximum aggregated DL-PRS bandwidth in MHz for FR2, which is supported and reported by UE.  **- *maximumOfDL-PRS-BandwidthPerPFL-FR1***: Indicates the maximum DL-PRS bandwidth in MHz for FR1, per PFL  **- *maximumOfDL-PRS-BandwidthPerPFL-FR2***: Indicates the maximum DL-PRS bandwidth in MHz for FR2, per PFL  **- *dl-PRS-BufferTypeOfBWA***: Indicates the DL-PRS buffering capability.  **- *prs-durationOfThreePRS-BWA-Processing***: Indicates the duration of DL-PRS symbols N in units of ms a UE can process every T ms assuming maximum aggregated DL-PRS bandwidth in MHz, which is supported and reported by UE.  **- *prs-durationOfThreePRS-BWA-ProcessingSymbolsN***: This field specifies the values for N. Enumerated values indicate 0.125, 0.25, 0.5, 1, 2, 4, 6, 8, 12, 16, 20, 25, 30, 32, 35, 40, 45, 50 ms.  **- *prs-durationOfThreePRS-BWA-ProcessingSymbolsT***: This field specifies the values for T. Enumerated values indicate 8, 16, 20, 30, 40, 80, 160, 320, 640, 1280, 3840 ms.  **- *maxNumOfAggregatedDL-PRS-ResourcePerSlot-FR1***: Indicates the Maximum number of aggregated DL-PRS Resources across aggregated PFLs that UE can process in a slot for FR1.  **- *maxNumOfAggregatedDL-PRS-ResourcePerSlot-FR2***: Indicates the Maximum number of aggregated DL-PRS Resources across aggregated PFLs that UE can process in a slot for FR2.  The UE can include this field only if the UE supports *prs-BWA-TwoContiguousIntrabandInMG-RRC-Connected****.*** Otherwise, the UE does not include this field.  NOTE15: *dl-PRS-BufferTypeOfBWA* follows buffering capability type reported in *dl-PRS-BufferType.*  NOTE16: The value N should be equal or smaller than the value N reported by *durationOfPRS-ProcessingSymbols*, or this value T should be equal or larger than the value T reported by *durationOfPRS-ProcessingSymbolsInEveryTms.*  NOTE17: Each three linked DL-PRS Resources are counted as 1 resource.  NOTE18: *maxNumOfAggregatedDL-PRS-ResourcePerSlot* should be equal or smaller than the value reported by *maxNumOfDL-PRS-ResProcessedPerSlot*.  NOTE19: The above parameters are reported assuming a configured measurement gap and a maximum ratio of measurement gap length (MGL)/measurement gap repetition period (MGRP) of no more than 30%. |
| ***prs-BWA-TwoContiguousIntraband-RRC-IdleAndInactive***  Indicates the UE capability for support of DL-PRS processing capabilities for aggregated DL-PRS processing of 2 PFLs in intra-band contiguous for RRC\_INACTIVE and RRC\_IDLE state.  The UE can include this field only if the UE supports *dl-PRS-BufferType-RRC-Inactive, durationOfPRS-Processing-RRC-Inactive and maxNumOfDL-PRS-ResProcessedPerSlot-RRC-Inactive*. Otherwise, the UE does not include this field. The capability signalling comprises the following parameters:  - ***maximumOfTwoAggregatedDL-PRS-Bandwidth-FR1***: Indicates the maximum aggregated DL-PRS bandwidth in MHz for FR1, which is supported and reported by UE.  - ***maximumOfTwoAggregatedDL-PRS-Bandwidth-FR2***: Indicates the maximum aggregated DL-PRS bandwidth in MHz for FR2, which is supported and reported by UE.  - ***maximumOfDL-PRS-BandwidthPerPFL-FR1***: Indicates the maximum DL-PRS bandwidth in MHz for FR1, per PFL.  - ***maximumOfDL-PRS-BandwidthPerPFL-FR2***: Indicates the maximum DL-PRS bandwidth in MHz for FR2, per PFL.  - ***dl-PRS-BufferTypeOfBWA***: Indicates the DL-PRS buffering capability.  - ***prs-durationOfTwoPRS-BWA-Processing***: Indicates the duration of DL-PRS symbols N in units of ms a UE can process every T ms assuming maximum aggregated DL-PRS bandwidth in MHz, which is supported and reported by UE.  - ***prs-durationOfTwoPRS-BWA-ProcessingSymbolsN***: This field specifies the values for N. Enumerated values indicate 0.125, 0.25, 0.5, 1, 2, 4, 6, 8, 12, 16, 20, 25, 30, 32, 35, 40, 45, 50 ms.  - ***prs-durationOfTwoPRS-BWA-ProcessingSymbolsT***: This field specifies the values for T. Enumerated values indicate 8, 16, 20, 30, 40, 80, 160, 320, 640, 1280, 2560 ms.  - ***maxNumOfAggregatedDL-PRS-ResourcePerSlot-FR1***: Indicates the Maximum number of aggregated DL-PRS Resources across aggregated PFLs that UE can process in a slot for FR1.  - ***maxNumOfAggregatedDL-PRS-ResourcePerSlot-FR2***: Indicates the Maximum number of aggregated DL-PRS Resources across aggregated PFLs that UE can process in a slot for FR2.  NOTE 20: *dl-PRS-BufferTypeOfBWA* follows buffering capability type reported in *dl-PRS-BufferType.*  NOTE 21: The value N should be equal or smaller than the value N reported by *durationOfPRS-ProcessingSymbols*, or this value T should be equal or larger than the value T reported by *durationOfPRS-ProcessingSymbolsInEveryTms.*  NOTE 22: Each two linked DL-PRS resources are counted as 1 resource.  NOTE 23: *maxNumOfAggregatedDL-PRS-ResourcePerSlot* should be equal or smaller than the value reported by *maxNumOfDL-PRS-ResProcessedPerSlot-RRC-Inactive.* |
| ***prs-BWA-ThreeContiguousIntraband-RRC-IdleAndInactive***  Indicates the UE capability for support of DL-PRS processing capabilities for aggregated DL-PRS processing of 3 PFLs in intra-band contiguous for RRC\_INACTIVE and RRC\_IDLE state. The UE can include this field only if the UE supports *prs-BWA-TwoContiguousIntraband-RRC-IdleAndInactive*. Otherwise, the UE does not include this field. The capability signalling comprises the following parameters:  **- *maximumOfThreeAggregatedDL-PRS-Bandwidth-FR1***: Indicates the maximum aggregated DL-PRS bandwidth in MHz of for FR1, which is supported and reported by UE.  **- *maximumOfThreeAggregatedDL-PRS-Bandwidth-FR2***: Indicates the maximum aggregated DL-PRS bandwidth in MHz for FR2, which is supported and reported by UE.  **- *maximumOfDL-PRS-BandwidthPerPFL-FR1***: Indicates the maximum DL-PRS bandwidth in MHz for FR1, per PFL  **- *maximumOfDL-PRS-BandwidthPerPFL-FR2***: Indicates the maximum DL-PRS bandwidth in MHz for FR2, per PFL  **- *dl-PRS-BufferTypeOfBWA***: Indicates the DL-PRS buffering capability.  **- *prs-durationOfThreePRS-BWA-Processing***: Indicates the duration of DL-PRS symbols N in units of ms a UE can process every T ms assuming maximum aggregated DL-PRS bandwidth in MHz, which is supported and reported by UE.  **- *prs-durationOfThreePRS-BWA-ProcessingSymbolsN***: This field specifies the values for N. Enumerated values indicate 0.125, 0.25, 0.5, 1, 2, 4, 6, 8, 12, 16, 20, 25, 30, 32, 35, 40, 45, 50 ms.  **- *prs-durationOfThreePRS-BWA-ProcessingSymbolsT***: This field specifies the values for T. Enumerated values indicate 8, 16, 20, 30, 40, 80, 160, 320, 640, 1280, 3840 ms.  **- *maxNumOfAggregatedDL-PRS-ResourcePerSlot-FR1***: Indicates the Maximum number of aggregated DL-PRS Resources across aggregated PFLs that UE can process in a slot for FR1.  **- *maxNumOfAggregatedDL-PRS-ResourcePerSlot-FR2***: Indicates the Maximum number of aggregated DL-PRS Resources across aggregated PFLs that UE can process in a slot for FR2.  NOTE 24: *dl-PRS-BufferTypeOfBWA* follows buffering capability type reported in *dl-PRS-BufferType.*  NOTE 25: The value N should be equal or smaller than the value N reported by *durationOfPRS-ProcessingSymbols*, or this value T should be equal or larger than the value T reported by *durationOfPRS-ProcessingSymbolsInEveryTms.*  NOTE 26: Each two linked DL-PRS resources are counted as 1 resource.  NOTE 27: *maxNumOfAggregatedDL-PRS-ResourcePerSlot* should be equal or smaller than the value reported by *maxNumOfDL-PRS-ResProcessedPerSlot-RRC-Inactive.* |
| ***reducedNumOfSampleInMeasurementWithPRS-BWA-RRC-Connected***  Indicates whether the UE supports reduced number of samples in positioning measurements with DL-PRS bandwidth aggregation for RRC\_CONNECTED. The UE can include this field only if the UE indicates the capability of maximum aggregated DL-PRS bandwidth for the supported FR1 or FR2 bands by using *maximumOfTwoAggregatedDL-PRS-Bandwidth-FR1* or *maximumOfTwoAggregatedDL-PRS-Bandwidth-FR2* of *prs-BWA-TwoContiguousIntrabandInMG-RRC-Connected****.*** Otherwise, the UE does not include this field. |
| ***reducedNumOfSampleInMeasurementWithPRS-BWA-RRC-IdleAndInactive***  Indicates whether the UE supports reduced number of samples in positioning measurements with DL-PRS bandwidth aggregation for RRC\_IDLE and RRC\_INACTIVE. The UE can include this field only if the UE indicates the capability of maximum aggregated DL-PRS bandwidth for the supported FR1 or FR2 bands by using *maximumOfTwoAggregatedDL-PRS-Bandwidth-FR1* or *maximumOfTwoAggregatedDL-PRS-Bandwidth-FR2* of *prs-BWA-TwoContiguousIntrabandInMG-RRC-Connected****.*** Otherwise, the UE does not include this field. |
| ***dl-PRS-MeasurementWithRxFH-RRC-Inactive***  Indicates the UE capability for support of DL-PRS measurement with Rx frequency hopping in RRC\_INACTIVE for RedCap UEs. The UE can include this field only if the UE supports *dl-PRS-MeasurementWithRxFH-RRC-Connected* and *prs-ProcessingRRC-Inactive* defined in TS 38.331 [35]. Otherwise, the UE does not include this field. |
| ***dl-PRS-MeasurementWithRxFH-RRC-Idle***  Indicates the UE capability for support of DL-PRS measurement with Rx frequency hopping in RRC\_IDLE for RedCap UEs. The UE can include this field only if the UE supports *dl-PRS-MeasurementWithRxFH-RRC-Connected*. Otherwise, the UE does not include this field. |
| ***reducedNumOfSampleForMeasurementWithFH-RRC-Connected***  Indicates whether the UE supports reduced number of samples for DL-PRS based positioning measurements with frequency hopping for RRC\_CONNECTED. The UE can include this field only if the UE supports *supportOfRedCap* or *supportOfERedCap* defined in TS 38.331 [35]*,* *supportedDL-PRS-ProcessingSamples-RRC-CONNECTED* and *dl-PRS-MeasurementWithRxFH-RRC-Connected*. Otherwise, the UE does not include this field. |
| ***reducedNumOfSampleForMeasurementWithFH-RRC-IdleAndInactive***  Indicates whether the UE supports reduced number of samples for DL-PRS based positioning measurements with frequency hopping for RRC\_IDLE and RRC\_INACTIVE. The UE can include this field only if the UE supports *supportOfRedCap* or *supportOfERedCap* defined in TS 38.331 [35], *supportedDL-PRS-ProcessingSamples-RRC-CONNECTED* and *dl-PRS-MeasurementWithRxFH-RRC-Connected*. Otherwise, the UE does not include this field. |
| ***supportOfPRS-BWA-WithTwoPFL-Combination***  Indicates whether the UE supports DL-PRS bandwidth aggregation with two PFL combinations. The UE can include this field only if the UE supports *prs-BWA-TwoContiguousIntrabandInMG-RRC-Connected*. Otherwise, the UE does not include this field. |
| ***dl-PRS-MeasurementWithRxFH-RRC-Connected***  Indicates the UE capability for DL-PRS measurement with Rx frequency hopping within a MG and measurement reporting in RRC\_CONNECTED for RedCap UEs. The UE can include this field only if the UE supports *supportedBandwidthPRS*, *dl-PRS-BufferType*, *durationOfPRS-Processing*, *maxNumOfDL-PRS-ResProcessedPerSlot* and one of *supportOfRedCap* and *supportOfERedCap* defined in TS 38.331 [35]. Otherwise, the UE does not include this field. The capability signalling comprises the following parameters:  - ***maximumPRS-BandwidthAcrossAllHopsFR1:*** Indicates the maximum DL-PRS bandwidth across all hops in MHz for FR1, which is supported and reported by UE.  - ***maximumPRS-BandwidthAcrossAllHopsFR2***: Indicates the maximum DL-PRS bandwidth across all hops in MHz for FR2, which is supported and reported by UE.  - ***maximumFH-Hops***: Indicates the maximum number of hops, which is supported and reported by UE.  - ***processingDuration***: Indicates the duration of DL-PRS symbols N3 in units of ms a UE can process every T3 ms.  - ***processingPRS-SymbolsDurationN3***: This field specifies the values for N3. Enumerated values indicate 0.125, 0.25, 0.5, 1, 2, 4, 6, 8, 12, 16, 20, 25, 30, 32, 35, 40, 45, 50 ms.  - ***processingDurationT3***: This field specifies the values for T3. Enumerated values indicate 8, 16, 20, 30, 40, 80, 160, 320, 640, 1280ms.  - ***rf-RxRetuneTimeFR1***: Indicates the RF Rx retune times between consecutive hops for FR1. Enumerated values indicate 70, 140, 210µs.  - ***rf-RxRetuneTimeFR2***: Indicates the RF Rx retune times between consecutive hops for FR2. Enumerated values indicate 35, 70, 140µs.  - ***numOfOverlappingPRB***: Indicates the overlapping PRB(s) between adjacent hops. Enumerated values indicate 0,1,2,4 PRBs.  NOTE 28: The maximum DL-PRS bandwidth per hop follows *supportedBandwidthPRS*.  NOTE 29: DL-PRS buffering capability follows *dl-PRS-BufferType*. |
| NOTE 9: When the target device provides the *durationOfPRS-Processing* capability (*N*, *T*) for any time window defined in TS 38.214 [45] clause 5.1.6.5, the target device should be capable of processing all DL-PRS Resources within , if  - where K is defined in the TS 38.214 [45] clause 5.1.6.5, and  - the number of DL-PRS Resources in each slot does not exceed the *maxNumOfDL-PRS-ResProcessedPerSlot*, and  - the configured measurement gap and a maximum ratio of measurement gap length (MGL) / measurement gap repetition period (MGRP) is as specified in TS 38.133 [46]. |

#### *– NR-DL-PRS-QCL-ProcessingCapability*

The IE *NR-DL-PRS-QCL-ProcessingCapability* defines the common UE DL-PRS QCL Processing capability. The UE can include this IE only if the UE supports *NR-DL-PRS-ProcessingCapability*. Otherwise, the UE does not include this IE.

In the case of capabilities for multiple NR positioning methods are provided, the IE *NR-DL-PRS-QCL-ProcessingCapability* applies across the NR positioning methods and the target device shall indicate the same values for the capabilities in IEs *NR-DL-TDOA-ProvideCapabilities*, *NR-DL-AoD-ProvideCapabilities*, and *NR-Multi-RTT-ProvideCapabilities*.

Editor's Note: It is FFS whether the *NR-DL-PRS-QCL-ProcessingCapability* is also needed for AI/ML positioning.

-- ASN1START

NR-DL-PRS-QCL-ProcessingCapability-r16 ::= SEQUENCE {

dl-PRS-QCL-ProcessingCapabilityBandList-r16 SEQUENCE (SIZE (1..nrMaxBands-r16)) OF

DL-PRS-QCL-ProcessingCapabilityPerBand-r16,

...

}

DL-PRS-QCL-ProcessingCapabilityPerBand-r16 ::= SEQUENCE {

freqBandIndicatorNR-r16 FreqBandIndicatorNR-r16,

ssb-FromNeighCellAsQCL-r16 ENUMERATED { supported} OPTIONAL,

prs-FromServNeighCellAsQCL-r16 ENUMERATED { supported} OPTIONAL,

...

}

-- ASN1STOP

| *NR-DL-PRS-QCL-ProcessingCapability* field descriptions |
| --- |
| ***ssb-FromNeighCellAsQCL***  Indicates the support of SSB from neighbour cell as QCL source of a DL-PRS. UE supporting this feature also support reusing SSB measurement from RRM for receiving DL-PRS.  Note: It refers to Type-C for FR1 and Type-C & Type-D support for FR2. |
| ***prs-FromServNeighCellAsQCL***  Indicates the support of DL-PRS from serving/neighbour cell as QCL source of a DL-PRS.  Note 1: It refers to Type-D support for FR2.  Note 2: A DL-PRS from a PRS-only TP is treated as DL-PRS from a non-serving cell. |

#### – *NR-DL-PRS-ResourceID*

The IE *NR-DL-PRS-ResourceID* defines the identity of a DL-PRS Resource of a DL-PRS Resource Set of a TRP.

-- ASN1START

NR-DL-PRS-ResourceID-r16 ::= INTEGER (0..nrMaxNumDL-PRS-ResourcesPerSet-1-r16)

-- ASN1STOP

#### *– NR-DL-PRS-ResourcesCapability*

The IE *NR-DL-PRS-ResourcesCapability* defines the DL-PRS Resources capability for each positioning method. The UE can include this IE only if the UE supports *NR-DL-PRS-ProcessingCapability*. Otherwise, the UE does not include this IE.

Editor's Note: It is FFS whether the *NR-DL-PRS-ResourcesCapability* is also needed for AI/ML positioning.

-- ASN1START

NR-DL-PRS-ResourcesCapability-r16 ::= SEQUENCE {

maxNrOfDL-PRS-ResourceSetPerTrpPerFrequencyLayer-r16

INTEGER (1..2),

maxNrOfTRP-AcrossFreqs-r16 ENUMERATED { n4, n6, n12, n16, n32,

n64, n128, n256, ..., n24-v1690},

maxNrOfPosLayer-r16 INTEGER (1..4),

dl-PRS-ResourcesCapabilityBandList-r16 SEQUENCE (SIZE (1..nrMaxBands-r16)) OF

DL-PRS-ResourcesCapabilityPerBand-r16,

dl-PRS-ResourcesBandCombinationList-r16 DL-PRS-ResourcesBandCombinationList-r16,

...

}

DL-PRS-ResourcesCapabilityPerBand-r16 ::= SEQUENCE {

freqBandIndicatorNR-r16 FreqBandIndicatorNR-r16,

maxNrOfDL-PRS-ResourcesPerResourceSet-r16 ENUMERATED { n1, n2, n4, n8, n16, n32, n64, ...},

maxNrOfDL-PRS-ResourcesPerPositioningFrequencylayer-r16

ENUMERATED { n6, n24, n32, n64, n96, n128,

n256, n512, n1024, ...},

...

}

DL-PRS-ResourcesBandCombinationList-r16 ::= SEQUENCE (SIZE (1..maxBandComb-r16)) OF

DL-PRS-ResourcesBandCombination-r16

DL-PRS-ResourcesBandCombination-r16 ::= SEQUENCE {

bandList-r16 SEQUENCE (SIZE (1..maxSimultaneousBands-r16)) OF

FreqBandIndicatorNR-r16,

maxNrOfDL-PRS-ResourcesAcrossAllFL-TRP-ResourceSet-r16

CHOICE {

fr1-Only-r16 ENUMERATED {n6, n24, n64, n128, n192,

n256, n512, n1024, n2048},

fr2-Only-r16 ENUMERATED {n24, n64, n96, n128, n192,

n256, n512, n1024, n2048},

fr1-FR2Mix-r16 SEQUENCE {

fr1-r16 ENUMERATED {n6, n24, n64, n96, n128,

n192, n256, n512, n1024, n2048},

fr2-r16 ENUMERATED {n24, n64, n96, n128, n192,

n256, n512, n1024, n2048},

...

},

...

},

...

}

-- ASN1STOP

| *NR-DL-PRS-ResourcesCapability* field descriptions |
| --- |
| ***maxNrOfDL-PRS-ResourceSetPerTrpPerFrequencyLayer***  Indicates the maximum number of DL-PRS Resource Sets per TRP per positioning frequency layer supported by UE. |
| ***maxNrOfTRP-AcrossFreqs***  Indicates the maximum number of TRPs across all positioning frequency layers. |
| ***maxNrOfPosLayer***  Indicates the maximum number of supported positioning frequency layers. |
| ***dl-PRS-ResourcesBandCombinationList***  Provides the capabilities of DL-PRS Resources for the indicated band combination in *bandList*. This field is provided for all band combinations for which the target device supports DL-PRS. |
| ***maxNrOfDL-PRS-ResourcesPerResourceSet***  Indicates the maximum number of DL-PRS Resources per DL-PRS Resource Set. Value 16, 32, 64 are only applicable to FR2 bands. Value 1 is not applicable for DL-AoD. |
| ***maxNrOfDL-PRS-ResourcesPerPositioningFrequencylayer***  Indicates the maximum number of DL-PRS Resources per positioning frequency layer. Value 6 is only applicable to FR1 bands. |
| ***maxNrOfDL-PRS-ResourcesAcrossAllFL-TRP-ResourceSet***  Indicates the maximum number of DL-PRS Resources supported by UE across all frequency layers, TRPs and DL-PRS Resource Sets.  fr1-Only: This is applicable for FR1 only band combinations;  fr2-Only: This is applicable for FR2 only band combinations;  fr1-FR2Mix: This is applicable for band combinations containing FR1 and FR2 bands. fr1 means for FR1 in FR1/FR2 mixed operation, and fr2 means for FR2 in FR1/FR2 mixed operation. |

#### – *NR-DL-PRS-ResourceSetID*

The IE *NR-DL-PRS-ResourceSetID* defines the identity of a DL-PRS Resource Set of a TRP.

-- ASN1START

NR-DL-PRS-ResourceSetID-r16 ::= INTEGER (0..nrMaxNumDL-PRS-ResourceSetsPerTRP-1-r16)

-- ASN1STOP

#### – *NR-DL-PRS-TRP-TEG-Info*

The IE *NR-DL-PRS-TRP-TEG-Info* is used by the location server to provide the association information of DL-PRS Resources with TRP Tx TEGs.

-- ASN1START

NR-DL-PRS-TRP-TEG-Info-r17 ::= SEQUENCE (SIZE (1..nrMaxFreqLayers-r16)) OF

NR-DL-PRS-TRP-TEG-InfoPerFreqLayer-r17

NR-DL-PRS-TRP-TEG-InfoPerFreqLayer-r17 ::= SEQUENCE (SIZE (1..nrMaxTRPsPerFreq-r16)) OF

NR-DL-PRS-TRP-TEG-InfoPerTRP-r17

NR-DL-PRS-TRP-TEG-InfoPerTRP-r17 ::= SEQUENCE {

dl-PRS-ID-r17 INTEGER (0..255),

nr-PhysCellID-r17 NR-PhysCellID-r16 OPTIONAL, -- Need ON

nr-CellGlobalID-r17 NCGI-r15 OPTIONAL, -- Need ON

nr-ARFCN-r17 ARFCN-ValueNR-r15 OPTIONAL, -- Need ON

dl-PRS-TEG-InfoSet-r17 SEQUENCE (SIZE(1..nrMaxSetsPerTrpPerFreqLayer-r16)) OF

DL-PRS-TEG-InfoPerResourceSet-r17,

...,

[[

nr-TRP-TxTEG-TimingErrorMargin-r17 TEG-TimingErrorMargin-r17 OPTIONAL -- Need ON

]]

}

DL-PRS-TEG-InfoPerResourceSet-r17 ::= SEQUENCE (SIZE(1..nrMaxResourcesPerSet-r16)) OF

DL-PRS-TEG-InfoElement-r17

DL-PRS-TEG-InfoElement-r17 ::= SEQUENCE {

dl-prs-trp-Tx-TEG-ID-r17 INTEGER (0..maxNumOfTRP-TxTEGs-1-r17),

...

}

-- ASN1STOP

|  |
| --- |
| *NR-DL-PRS-TRP-TEG-Info* field descriptions |
| ***dl-PRS-ID***  This field specifies the DL-PRS ID of the TRP for which the TRP Tx TEG information is provided. |
| ***nr-PhysCellID***  This field specifies the physical Cell-ID of the TRP for which the TRP Tx TEG information is provided, as defined in TS 38.331 [35]. |
| ***nr-CellGlobalID***  This field specifies the NCGI, the globally unique identity of a cell in NR, of the TRP for which the TRP Tx TEG information is provided, as defined in TS 38.331 [35]. |
| ***nr-ARFCN***  This field specifies the NR-ARFCN of the TRP's CD-SSB (as defined in TS 38.300 [47]) corresponding to *nr-PhysCellID*. |
| ***dl-PRS-TEG-InfoSet***  This field specifies the TRP Tx TEG ID associated with the transmissions of each DL-PRS Resource of the TRP. The *dl-prs-trp-Tx-TEG-ID* in *dl-PRS-TEG-InfoSet* is associated with the *nr-DL-PRS-ResourceID* of *NR-DL-PRS-Info* using the same structure and order. |
| ***nr-TRP-TxTEG-TimingErrorMargin***  This field specifies the timing error margin value for all the TRP Tx TEGs contained within one *NR-DL-PRS-TRP-TEG-InfoPerTRP*. |

#### – *NR-IntegrityRiskParameters*

The IE *NR-IntegrityRiskParameters* is used by the location server to indicate the residual risks to UE.

-- ASN1START

NR-IntegrityRiskParameters-r18 ::= SEQUENCE {

nr-ProbOnsetTRP-Fault-r18 INTEGER (0..255),

nr-MeanTRP-FaultDuration-r18 INTEGER (1..3600),

...

}

-- ASN1STOP

|  |
| --- |
| *NR-IntegrityRiskParameters* field descriptions |
| ***nr-ProbOnsetTRP-Fault***  This field specifies the Probability of Onset of TRP Fault per Time Unit which is the probability of occurrence of TRP error to exceed the error bound for more than the Time to Alert (TTA).  This field specifies the onset probability that the error exceeds a bound created using the minimum allowed inflation factor *Kmin*, and bounding parameters as *mean* + *Kmin* \* *stdDev* where *Kmin* = *normInv*(*irMaximum* / 2), with *irMaximum* as provided in IE *nr-IntegrityServiceParameters*.  The probability is calculated by *P*=10-0.04*n* [hour-1] where *n* is the value of *nr-ProbOnsetTRP-Fault* and the range is 10-10.2 to 1 per hour. |
| ***nr-MeanTRP-FaultDuration***  This field specifies the Mean TRP Fault Duration which is the mean duration between when a TRP fault occurs, and the user is alerted by IE *NR-IntegrityServiceAlert* (or the integrity violation is over).  Scale factor 1 s; range 1-3600 s. |

#### – *NR-IntegrityServiceAlert*

The IE *NR-IntegrityServiceAlert* is used by the location server to indicate whether the corresponding assistance data can be used for integrity related applications.

-- ASN1START

NR-IntegrityServiceAlert-r18 ::= SEQUENCE (SIZE (1..nrMaxFreqLayers-r16)) OF

NR-TRP-IntegrityServiceAlertPerFreqLayer-r18

NR-TRP-IntegrityServiceAlertPerFreqLayer-r18 ::= SEQUENCE (SIZE (1..nrMaxTRPsPerFreq-r16))

OF NR-TRP-IntegrityServiceAlertElement-r18

NR-TRP-IntegrityServiceAlertElement-r18 ::= SEQUENCE {

dl-PRS-ID-r18 INTEGER (0..255),

nr-PhysCellID-r18 NR-PhysCellID-r16 OPTIONAL, -- Need ON

nr-CellGlobalID-r18 NCGI-r15 OPTIONAL, -- Need ON

nr-ARFCN-r18 ARFCN-ValueNR-r15 OPTIONAL, -- Need ON

rtd-DoNotUse-r18 BOOLEAN OPTIONAL, -- Need OR

trp-LocationDoNotUse-r18 BOOLEAN OPTIONAL, -- Need OR

beamInfo-DoNotUse-r18 BOOLEAN OPTIONAL, -- Need OR

beamAntennaInfo-DoNotUse-r18 BOOLEAN OPTIONAL, -- Need OR

...

}

-- ASN1STOP

|  |
| --- |
| *NR-IntegrityServiceAlert* field descriptions |
| ***nr-PhysCellID***  This field specifies the physical cell identity of the associated TRP, as defined in TS 38.331 [35]. |
| ***nr-CellGlobalID***  This field specifies the NCGI, the globally unique identity of a cell in NR, of the associated TRP, as defined in TS 38.331 [35]. The server should include this field if it considers that it is needed to resolve ambiguity in the TRP indicated by *nr-PhysCellID*. |
| ***nr-ARFCN***  This field specifies the NR-ARFCN of the TRP's CD-SSB (as defined in TS 38.300 [47]) corresponding to *nr-PhysCellID*. |
| ***rtd-DoNotUse***  This field indicates whether the RTD info in IE *NR-RTD-Info* can be used for integrity related applications (FALSE) or not (TRUE). |
| ***trp-LocationDoNotUse***  This field indicates whether the TRP/ARP location in IE *NR-TRP-LocationInfo* can be used for integrity related applications (FALSE) or not (TRUE). |
| ***beamInfo-DoNotUse***  This field indicates whether the spatial direction information in IE *NR-DL-PRS-BeamInfo* can be used for integrity related applications (FALSE) or not (TRUE). |
| ***beamAntennaInfo-DoNotUse***  This field indicates whether the beam antenna information in IE *NR-TRP-BeamAntennaInfo* can be used for integrity related applications (FALSE) or not (TRUE). |

#### – *NR-IntegrityServiceParameters*

The IE *NR-IntegrityServiceParameters* is used by the location server to provide the range of Integrity Risk (IR) for which the integrity assistance data are valid.

-- ASN1START

NR-IntegrityServiceParameters-r18 ::= SEQUENCE {

ir-Minimum-r18 INTEGER (0..255),

ir-Maximum-r18 INTEGER (0..255),

...

}

-- ASN1STOP

|  |
| --- |
| *NR-IntegrityServiceParameters* field descriptions |
| ***ir-Minimum***  This field specifies the Minimum Integrity Risk (IR) which is the minimum IR for which the error bounds provided in the IEs *NR-IntegrityRTD-InfoBounds*, *NR-IntegrityBeamInfoBounds*, *NR-IntegrityBeamPowerBounds*, and *NR-IntegrityLocationBounds* are valid.  The IR is calculated by where n is the value of *ir-Minimum* and the range is 10-10.2 to 1. |
| ***ir-Maximum***  This field specifies the Maximum Integrity Risk (IR) which is the maximum IR for which the error bounds provided in the IEs *NR-IntegrityRTD-InfoBounds*, *NR-IntegrityBeamInfoBounds*, *NR-IntegrityBeamPowerBounds*, and *NR-IntegrityLocationBounds* are valid.  The IR is calculated by where n is the value of *ir-Maximum* and the range is 10-10.2 to 1. |

#### *– NR-On-Demand-DL-PRS-Configurations*

The IE *NR-On-Demand-DL-PRS-Configurations* provides a set of possible DL-PRS configurations which can be requested by the target device on-demand.

-- ASN1START

NR-On-Demand-DL-PRS-Configurations-r17 ::= SEQUENCE {

on-demand-dl-prs-configuration-list-r17 SEQUENCE (SIZE (1..maxOD-DL-PRS-Configs-r17)) OF

On-Demand-DL-PRS-Configuration-r17,

...,

[[

onDemandDL-PRS-AggregationList-r18 SEQUENCE (SIZE (1.. maxOD-DL-PRS-Configs-r17)) OF

OnDemandDL-PRS-AggregationInfo-r18 OPTIONAL-- Need OR

]]

}

On-Demand-DL-PRS-Configuration-r17 ::= SEQUENCE {

dl-prs-configuration-id-r17 DL-PRS-Configuration-ID-r17,

nr-DL-PRS-PositioningFrequencyLayer-r17 NR-DL-PRS-PositioningFrequencyLayer-r16,

nr-DL-PRS-Info-r17 NR-DL-PRS-Info-r16,

...

}

DL-PRS-Configuration-ID-r17 ::= SEQUENCE {

nr-dl-prs-configuration-id-r17 INTEGER (1..maxOD-DL-PRS-Configs-r17),

...

}

OnDemandDL-PRS-AggregationInfo-r18 ::= SEQUENCE (SIZE (2..3)) OF DL-PRS-Configuration-ID-r17

-- ASN1STOP

| *NR-On-Demand-DL-PRS-Configurations* field descriptions |
| --- |
| ***dl-prs-configuration-id***  This field identifies an On-demand DL-PRS Configuration information*.* |
| ***nr-DL-PRS-PositioningFrequencyLayer***  This field, together with *nr-DL-PRS-Info*, provides the On-demand DL-PRS Configuration information.  Only the following fields in IE *NR-DL-PRS-PositioningFrequencyLayer* are applicable:  *dl-PRS-ResourceBandwidth*, *dl-PRS-CombSizeN.*  The target device shall ignore the remaining fields in IE *NR-DL-PRS-PositioningFrequencyLayer.* |
| ***nr-DL-PRS-Info***  This field, together with *nr-DL-PRS-PositioningFrequencyLayer*, provides the On-demand DL-PRS Configuration information. Only the following fields in IE *NR-DL-PRS-Info* are applicable:  DL-PRS periodicity in *dl-PRS-Periodicity-and-ResourceSetSlotOffset*, *dl-PRS-ResourceRepetitionFactor*, *dl-PRS-NumSymbols*, comb-size in *dl-PRS-CombSizeN-AndReOffset*, *dl-PRS-QCL-Info*.  The target device shall ignore the remaining fields in IE *NR-DL-PRS-Info.* |
| ***onDemandDL-PRS-AggregationList***  This field provides a list of DL-PRS bandwidth aggregation information where each entry of DL-PRS bandwidth aggregation information indicates the identities of 2 or 3 On-demand DL-PRS Configuration information for DL-PRS that are available for aggregation. |

#### – *NR-On-Demand-DL-PRS-Information*

The IE *NR-On-Demand-DL-PRS-Information* defines the requested on-demand DL-PRS.

-- ASN1START

NR-On-Demand-DL-PRS-Information-r17 ::= SEQUENCE (SIZE (1..nrMaxFreqLayers-r16)) OF

NR-On-Demand-DL-PRS-PerFreqLayer-r17

NR-On-Demand-DL-PRS-PerFreqLayer-r17 ::= SEQUENCE {

dl-prs-FrequencyRangeReq-r17 ENUMERATED { fr1, fr2, ...},

dl-prs-ResourceSetPeriodicityReq-r17 ENUMERATED { p4, p5, p8, p10, p16, p20, p32, p40,

p64, p80, p160, p320, p640, p1280, p2560,

p5120, p10240, p20480, p40960, p81920, ...,

p128-v1760, p256-v1760, p512-v1760}

OPTIONAL,

dl-prs-ResourceBandwidthReq-r17 INTEGER (1..63) OPTIONAL,

dl-prs-ResourceRepetitionFactorReq-r17 ENUMERATED {n2, n4, n6, n8, n16, n32, ...}

OPTIONAL,

dl-prs-NumSymbolsReq-r17 ENUMERATED {n2, n4, n6, n12, ..., n1-v1800} OPTIONAL,

dl-prs-CombSizeN-Req-r17 ENUMERATED {n2, n4, n6, n12, ...} OPTIONAL,

dl-prs-QCL-InformationReqTRPlist-r17 DL-PRS-QCL-InformationReqTRPlist-r17 OPTIONAL,

...

}

DL-PRS-QCL-InformationReqTRPlist-r17 ::= SEQUENCE (SIZE (1..nrMaxTRPsPerFreq-r16)) OF

DL-PRS-QCL-InformationReqPerTRP-r17

DL-PRS-QCL-InformationReqPerTRP-r17 ::= SEQUENCE {

dl-PRS-ID-r17 INTEGER (0..255),

nr-PhysCellID-r17 NR-PhysCellID-r16 OPTIONAL,

nr-CellGlobalID-r17 NCGI-r15 OPTIONAL,

nr-ARFCN-r17 ARFCN-ValueNR-r15 OPTIONAL,

dl-prs-QCL-InformationReqSet-r17 SEQUENCE (SIZE (1..nrMaxSetsPerTrpPerFreqLayer-r16)) OF

DL-PRS-QCL-InfoReq-r17,

...

}

DL-PRS-QCL-InfoReq-r17 ::= SEQUENCE {

nr-DL-PRS-ResourceSetID-r17 NR-DL-PRS-ResourceSetID-r16,

dl-prs-QCL-InformationReq-r17 CHOICE {

dl-prs-QCL-InfoRecPerResourceSet-r17 DL-PRS-QCL-Info-r16,

dl-prs-QCL-Info-requested-r17 NULL

},

...,

[[

dl-prs-QCL-InfoRecPerResource-r17 SEQUENCE (SIZE (1..nrMaxResourcesPerSet-r16)) OF

DL-PRS-QCL-Info-r16 OPTIONAL

]]

}

-- ASN1STOP

|  |
| --- |
| *NR-On-Demand-DL-PRS-Information* field descriptions |
| ***dl-prs-FrequencyRangeReq***  This field specifies the frequency range for which the on-demand DL-PRS is requested. |
| ***dl-prs-ResourceSetPeriodicityReq***  This field specifies the requested periodicity of the DL-PRS Resource Set in slots. The periodicity depends on the subcarrier spacing (SCS) and takes values  slots, where for SCS of 15, 30, 60 and 120 kHz respectively. μ refers to the SCS of SSB of target device's current primary cell. |
| ***dl-prs-ResourceBandwidthReq***  This field specifies the requested number of PRBs allocated for the DL-PRS Resource (allocated DL-PRS bandwidth) in multiples of 4 PRBs. Integer value 1 corresponds to 24 PRBs, value 2 corresponds to 28 PRBs, value 3 corresponds to 32 PRBs and so on. |
| ***dl-prs-ResourceRepetitionFactorReq***  This field specifies the requested DL-PRS Resource repetition. Enumerated values *n2*, *n4*, *n6*, *n8*, *n16*, *n32* correspond to 2, 4, 6, 8, 16, 32 resource repetitions, respectively. |
| ***dl-prs-NumSymbolsReq***  This field specifies the requested number of symbols per DL-PRS Resource within a slot. |
| ***dl-prs-CombSizeN-Req***  This field specifies the requested Resource Element spacing in each symbol of the DL-PRS Resource. |
| ***dl-prs-QCL-InformationReqTRPlist***  This field specifies the recommended or requested QCL indication with other DL reference signals.  - ***dl-PRS-ID*** indicates the DL-PRS ID of the TRP for which the QCL information is recommended.  - ***nr-PhysCellID*** indicates the physical Cell-ID of the TRP for which the QCL information is recommended, as defined in TS 38.331 [35].  - ***nr-CellGlobalID*** indicates the NCGI, the globally unique identity of a cell in NR, of the TRP for which the QCL information is recommended, as defined in TS 38.331 [35].  - ***nr-ARFCN*** indicates the NR-ARFCN of the TRP's CD-SSB (as defined in TS 38.300 [47]) corresponding to nr-PhysCellID.  - ***dl-prs-QCL-InformationReqSet*** indicates the recommended QCL information per DL-PRS Resource Set.  - ***nr-DL-PRS-ResourceSetID*** indicates the DL-PRS Resource Set ID for which the QCL information is recommended.  - ***dl-prs-QCL-InformationReq***  - ***dl-prs-QCL-InfoRecPerResourceSet*** indicates a single recommended QCL source for the DL-PRS Resource Set.  - ***dl-prs-QCL-Info-requested*** indicates that the UE requests to provide the QCL information in the assistance data.  - ***dl-prs-QCL-InfoRecPerResource*** indicates a list of recommended QCL sources for the DL-PRS Resource Set. If this field is present, the *dl-prs-QCL-InformationReg* shall be ignored by the receiver. |

#### – *NR-On-Demand-DL-PRS-Request*

The IE *NR-On-Demand-DL-PRS-Request* is used by the target device to request on-demand DL-PRS from a location server.

-- ASN1START

NR-On-Demand-DL-PRS-Request-r17 ::= SEQUENCE {

dl-prs-StartTime-and-Duration-r17 DL-PRS-StartTime-and-Duration-r17 OPTIONAL,

nr-on-demand-DL-PRS-Information-r17 NR-On-Demand-DL-PRS-Information-r17 OPTIONAL,

dl-prs-configuration-id-PrefList-r17 SEQUENCE (SIZE (1..maxOD-DL-PRS-Configs-r17)) OF   
 DL-PRS-Configuration-ID-r17 OPTIONAL,

...,

[[

dl-PRS-AggregationID-PrefList-r18 SEQUENCE (SIZE (1.. maxOD-DL-PRS-Configs-r17)) OF

INTEGER (1.. maxOD-DL-PRS-Configs-r17)

OPTIONAL,

nr-OnDemandDL-PRS-AggregationReqList-r18 SEQUENCE (SIZE (1.. maxOD-DL-PRS-Configs-r17)) OF

NR-OnDemandDL-PRS-AggregationReqElement-r18

OPTIONAL

]]

}

DL-PRS-StartTime-and-Duration-r17 ::= SEQUENCE {

dl-prs-start-time-r17 INTEGER (1..1024) OPTIONAL,

dl-prs-duration-r17 SEQUENCE {

seconds-r17 INTEGER (0..59) OPTIONAL,

minutes-r17 INTEGER (0..59) OPTIONAL,

hours-r17 INTEGER (0..23) OPTIONAL,

...

} OPTIONAL,

...

}

NR-OnDemandDL-PRS-AggregationReqElement-r18 ::= SEQUENCE (SIZE (2..3)) OF

INTEGER (1..nrMaxFreqLayers-r16)

-- ASN1STOP

|  |
| --- |
| *NR-On-Demand-DL-PRS-Request* field descriptions |
| ***dl-prs-StartTime-and-Duration***  This field specifies the requested start time and duration for the on-demand DL-PRS and comprises the following subfields:  - ***dl-prs-start-time*** specifies the desired start time for the requested DL-PRS. It indicates the time in seconds from the time the IE *NR-On-Demand-DL-PRS-Request* was received.  - ***dl-prs-duration*** specifies the desired duration of the requested DL-PRS. The desired duration is the sum of the *seconds*, *minutes*, *hours* fields. If this field is included, at least one of the *seconds*, *minutes*, *hours* fields shall be present. |
| ***nr-on-demand-DL-PRS-Information***  This field specifies the on-demand DL-PRS configuration information requested by the target device.  NOTE: If the network provided predefined on-demand DL-PRS configurations (*NR-On-Demand-DL-PRS-Configurations*), the target device can only request explicit parameters (*nr-on-demand-DL-PRS-Information*) within the scope of those configurations. |
| ***dl-prs-configuration-id-PrefList***  This field specifies the on-demand DL-PRS configuration associated with *DL-PRS-Configuration-ID* in IE *NR-On-Demand-DL-PRS-Configurations* the target device wishes to obtain in the order of preference. The first *DL-PRS-Configuration-ID* in the list is the most preferred configuration, the second *DL-PRS-Configuration-ID* the second most preferred, etc. |
| ***dl-PRS-AggregationID-PrefList***  This field specifies a list of identities i.e., *DL-PRS-Configuration-ID*, for On-demand DL-PRS Configuration information i.e., *On-Demand-DL-PRS-Configuration*, thatthe target device wishes to obtain, for DL-PRS aggregation, in the order of preference. The first integer value in the list is the most preferred On-demand DL-PRS Configuration information; the second integer value in the list is the second most preferred, etc. |
| ***nr-OnDemandDL-PRS-AggregationReqList***  This field specifies a list of DL-PRS for specific PFL combinations for which the DL-PRS information i.e., *NR-On-Demand-DL-PRS-Information*, is requested by the target device for DL-PRS aggregation, listed in the order of preference. The first *NR-OnDemandDL-PRS-AggregationReqElement* in the list is the most preferred PFL combination for DL-PRS aggregation; the second element in the list is the second most preferred, etc. |

#### – *NR-On-Demand-DL-PRS-Configurations-Selected-IndexList*

The IE *NR-On-Demand-DL-PRS-Configurations-Selected-IndexList* is used by the location server to provide the selected available on-demand DL-PRS configurations to the target device.

In the case of available on-demand DL-PRS configurations for multiple NR positioning methods are provided, the *NR-On-Demand-DL-PRS-Configurations* shall be present in only one of *NR-Multi-RTT-ProvideAssistanceData*, *NR-DL-AoD-ProvideAssistanceData*, *NR-DL-TDOA-ProvideAssistanceData*, or *NR-AI-ML-PositioningProvideAssistanceData*.

-- ASN1START

NR-On-Demand-DL-PRS-Configurations-Selected-IndexList-r17 ::=

SEQUENCE (SIZE (1..maxOD-DL-PRS-Configs-r17)) OF

DL-PRS-Configuration-ID-r17

-- ASN1STOP

Editor's Note: It is FFS whether on-demand PRS is applicable to AI/ML positioning.

#### *– NR-On-Demand-DL-PRS-Support*

The IE *NR-On-Demand-DL-PRS-Support* defines the target device's on-demand DL-PRS capabilities.

-- ASN1START

NR-On-Demand-DL-PRS-Support-r17 ::= SEQUENCE {

nr-on-demand-DL-PRS-InformationSup-r17 ENUMERATED { supported } OPTIONAL,

nr-on-demand-DL-PRS-ConfigurationsSup-r17 ENUMERATED { supported } OPTIONAL,

...

}

-- ASN1STOP

| *NR-On-Demand-DL-PRS-Support* field descriptions |
| --- |
| ***nr-on-demand-DL-PRS-InformationSup***  This field, if present, indicates that the target device supports the IE *NR-On-Demand-DL-PRS-Information* in IE *NR-On-Demand-DL-PRS-Request*. |
| ***nr-on-demand-DL-PRS-ConfigurationsSup***  This field, if present, specifies that the target device supports the *dl-prs-configuration-id-PrefList* in IE *NR-On-Demand-DL-PRS-Request*. |

#### *– NR-PeriodicAssistData*

The IE *NR-PeriodicAssistData* is used by the location server to provide control parameters for a periodic assistance data delivery session (e.g., interval and duration) to the target device for UE‑based carrier phase positioning.

NOTE: Omission of a particular assistance data type field in IE *NR-PeriodicAssistData* means that the location server does not provide this assistance data type in a data transaction of a periodic assistance data delivery session, as described in clauses 5.2.1a and 5.2.2a. Inclusion of no assistance data type fields in IE *NR-PeriodicAssistData* means that a periodic assistance data delivery session is terminated.

-- ASN1START

NR-PeriodicAssistData-r18 ::= SEQUENCE {

nr-PeriodicPRU-DL-Info-r18 NR-PeriodicControlParam-r18 OPTIONAL, -- Need ON

...

}

-- ASN1STOP

#### *– NR-PeriodicAssistDataReq*

The IE *NR-PeriodicAssistDataReq* is used by the target device to request periodic assistance data delivery from a location server.

-- ASN1START

NR-PeriodicAssistDataReq-r18 ::= SEQUENCE {

nr-PeriodicPRU-DL-InfoReq-r18 NR-PeriodicControlParam-r18 OPTIONAL, -- Cond pPRU

...

}

-- ASN1STOP

| *Conditional presence* | Explanation |
| --- | --- |
| *pPRU* | The field is mandatory present if the target device requests periodic *nr-PRU-DL-Info*; otherwise it is not present. |

#### – *NR-PeriodicControlParam*

The IE *NR-PeriodicControlParam* is used to specify control parameters for a periodic assistance data delivery.

-- ASN1START

NR-PeriodicControlParam-r18 ::= SEQUENCE {

deliveryAmount-r18 INTEGER (1..32),

deliveryInterval-r18 INTEGER (4..81920),

...

}

-- ASN1STOP

| *NR-PeriodicControlParam* field descriptions |
| --- |
| ***deliveryAmount***  This field specifies the number of periodic assistance data deliveries. Integer values *N*=1…31 correspond to an amount of 2*N*. Integer value *N*=32 indicates an 'infinite/indefinite' amount, which means that the assistance data delivery should continue until a LPP *Abort* message is received. |
| ***deliveryInterval***  This field specifies the interval between assistance data deliveries in milliseconds. |

#### *– NR-PositionCalculationAssistance*

The IE *NR-PositionCalculationAssistance* is used by the location server to provide assistance data including integrity information to enable UE‑based downlink positioning.

-- ASN1START

NR-PositionCalculationAssistance-r16 ::= SEQUENCE {

nr-TRP-LocationInfo-r16 NR-TRP-LocationInfo-r16 OPTIONAL, -- Need ON

nr-DL-PRS-BeamInfo-r16 NR-DL-PRS-BeamInfo-r16 OPTIONAL, -- Need ON

nr-RTD-Info-r16 NR-RTD-Info-r16 OPTIONAL, -- Need ON

...,

[[

nr-TRP-BeamAntennaInfo-r17 NR-TRP-BeamAntennaInfo-r17 OPTIONAL, -- Need ON

nr-DL-PRS-Expected-LOS-NLOS-Assistance-r17

NR-DL-PRS-ExpectedLOS-NLOS-Assistance-r17

OPTIONAL, -- Need ON

nr-DL-PRS-TRP-TEG-Info-r17 NR-DL-PRS-TRP-TEG-Info-r17 OPTIONAL -- Need ON

]],

[[

nr-IntegrityServiceParameters-r18 NR-IntegrityServiceParameters-r18 OPTIONAL, -- Need OR

nr-IntegrityServiceAlert-r18 NR-IntegrityServiceAlert-r18 OPTIONAL, -- Need OR

nr-IntegrityRiskParameters-r18 NR-IntegrityRiskParameters-r18 OPTIONAL, -- Need OR

nr-IntegrityParametersTRP-LocationInfo-r18 NR-IntegrityParametersTRP-LocationInfo-r18

OPTIONAL, -- Cond Integrity1

nr-IntegrityParametersDL-PRS-BeamInfo-r18

NR-IntegrityParametersDL-PRS-BeamInfo-r18

OPTIONAL, -- Cond Integrity2

nr-IntegrityParametersRTD-Info-r18 NR-IntegrityParametersRTD-Info-r18

OPTIONAL, -- Cond Integrity3

nr-IntegrityParametersTRP-BeamAntennaInfo-r18 NR-IntegrityParametersTRP-BeamAntennaInfo-r18

OPTIONAL, -- Cond Integrity4

nr-PRU-DL-Info-r18 NR-PRU-DL-Info-r18 OPTIONAL -- Need ON

]]

}

NR-IntegrityParametersTRP-LocationInfo-r18 ::= SEQUENCE {

trp-ErrorCorrelationTime-r18 INTEGER(0..255) OPTIONAL, -- Need ON

dl-PRS-ResourceSetARP-ErrorCorrelationTime-r18 INTEGER(0..255) OPTIONAL, -- Need ON

dl-PRS-ResourceARP-ErrorCorrelationTime-r18 INTEGER(0..255) OPTIONAL, -- Need ON

...

}

NR-IntegrityParametersDL-PRS-BeamInfo-r18 ::= SEQUENCE {

dl-PRS-BeamInfoErrorCorrelationTime-r18 INTEGER (0..255),

...

}

NR-IntegrityParametersRTD-Info-r18 ::= SEQUENCE {

rtd-ErrorCorrelationTime-r18 INTEGER (0..255),

...

}

NR-IntegrityParametersTRP-BeamAntennaInfo-r18 ::= SEQUENCE {

trp-BeamAntennaInfoErrorCorrelationTime-r18 INTEGER (0..255),

...

}

-- ASN1STOP

| Conditional presence | Explanation |
| --- | --- |
| *Integrity1* | The field is optionally present, need OR, if *nr-TRP-LocationInfo* is present and *nr-IntegrityTRP-LocationBounds* is present in IE *NR-TRP-LocationInfo;* otherwise it is not present. |
| *Integrity2* | The field is optionally present, need OR, if *nr-DL-PRS-BeamInfo* is present and *nr-IntegrityBeamInfoBounds* is present in IE *NR-DL-PRS-BeamInfo;* otherwise it is not present. |
| *Integrity3* | The field is optionally present, need OR, if *nr-RTD-Info* is present and *nr-IntegrityRTD-InfoBounds* is present in IE *NR-RTD-Info;* otherwise it is not present. |
| *Integrity4* | The field is optionally present, need OR, if *nr-TRP-BeamAntennaInfo* is present and *nr-IntegrityBeamPowerBounds* is present in IE *NR-TRP-BeamAntennaInfo;* otherwise it is not present. |

| *NR-PositionCalculationAssistance* field descriptions |
| --- |
| ***nr-TRP-LocationInfo***  This field provides the location coordinates of the TRPs and location coordinates of antenna reference points for DL-PRS Resource Set(s) and DL-PRS Resources of the TRPs. |
| ***nr-DL-PRS-BeamInfo***  This field provides the spatial directions of DL-PRS Resources for TRPs. |
| ***nr-RTD-Info***  This field provides the time synchronization information between the reference TRP and neighbour TRPs. |
| ***nr-TRP-BeamAntennaInfo***  This field provides the relative DL-PRS Resource power between DL-PRS Resources per angle per TRP. |
| ***nr-DL-PRS-ExpectedLOS-NLOS-Assistance***  This field provides the expected likelihood of a LOS propagation path from a TRP to the target device. The information is provided per TRP or per DL-PRS Resource. |
| ***nr-DL-PRS-TRP-TEG-Info***  This field provides the TRP Tx TEG ID associated with the transmission of each DL-PRS Resource of the TRP. |
| ***nr-IntegrityServiceParameters***  This field specifiesthe range of Integrity Risk (IR) for which the integrity assistance data are valid. |
| ***nr-IntegrityServiceAlert***  This field indicates whether the corresponding assistance data can be used for integrity related applications. |
| ***trp-ErrorCorrelationTime***  This field specifies the TRP Error Correlation Time which is the upper bound of the correlation time of the TRP error. The time is calculated using:  Range is 1-28,200 s. |
| ***dl-PRS-ResourceSetARP-ErrorCorrelationTime***  This field, if present, specifies the DL-PRS Resource Set ARP Error Correlation Time which is the upper bound of the correlation time of the DL-PRS Resource Set ARP error. The time is calculated using:  Range is 1-28,200 s. |
| ***dl-PRS-ResourceARP-ErrorCorrelationTime***  This field, if present, specifies the DL-PRS Resource ARP Error Correlation Time which is the upper bound of the correlation time of the DL-PRS Resource ARP error. The time is calculated using:  Range is 1-28,200 s. |
| ***rtd-ErrorCorrelationTime***  This field specifies the inter-TRP synchronization error Correlation Time which is the upper bound of the correlation time of the inter-TRP synchronization error. The correlation time is calculated using:  Where *i* is the value given by *rtdErrorCorrelationTime*. Range is 1-28,200 s. |
| ***dl-PRS-BeamInfoErrorCorrelationTime***  This field specifies the Beam Boresight Direction Angle Error Correlation Time which is the upper bound of the correlation time of the DL-PRS Resource angle error. The time is calculated using:  Range is 1-28,200 s. |
| ***trp-BeamAntennaInfoErrorCorrelationTime***  This field specifies the Mean Beam Power Error Correlation Time which is the upper bound of the correlation time of the mean beam power error.  The time is calculated using:  Range is 1-28,200 s. |
| ***nr-PRU-DL-Info***  This field provides the measurements reported by a PRU to the target UE. |

#### – *NR-PRU-DL-Info*

The IE *NR-PRU-DL-Info* is used by the location server to provide PRU measurements and additional information reported by a PRU for UE-based DL-TDOA and AI/ML positioning to a target UE.

Editor's Note: It is FFS whether IE *NR-PRU-DL-Info* is applicable to AI/ML positioning.

-- ASN1START

NR-PRU-DL-Info-r18 ::= SEQUENCE {

nr-PRU-LocationInfo-r18 LocationCoordinates OPTIONAL, -- Need ON

nr-PRU-DL-TDOA-MeasInfo-r18 NR-DL-TDOA-SignalMeasurementInformation-r16

OPTIONAL, -- Need ON

nr-PRU-DL-AoD-MeasInfo-r18 NR-DL-AoD-SignalMeasurementInformation-r16

OPTIONAL, -- Need ON

nr-PRU-RSCP-MeasInfo-r18 NR-PRU-RSCP-MeasurementInformation-r18

OPTIONAL, -- Need ON

...

}

NR-PRU-RSCP-MeasurementInformation-r18 ::= SEQUENCE (SIZE(1..nrMaxTRPs-r16)) OF

NR-PRU-RSCP-MeasElement-r18

NR-PRU-RSCP-MeasElement-r18 ::= SEQUENCE {

dl-PRS-ID-r18 INTEGER (0..255),

nr-PhysCellID-r18 NR-PhysCellID-r16 OPTIONAL, -- Need ON

nr-CellGlobalID-r18 NCGI-r15 OPTIONAL, -- Need ON

nr-ARFCN-r18 ARFCN-ValueNR-r15 OPTIONAL, -- Need ON

nr-DL-PRS-ResourceID-r18 NR-DL-PRS-ResourceID-r16 OPTIONAL, -- Need ON

nr-DL-PRS-ResourceSetID-r18 NR-DL-PRS-ResourceSetID-r16 OPTIONAL, -- Need ON

nr-TimeStamp-r18 NR-TimeStamp-r16,

nr-los-nlos-Indicator-r18 CHOICE {

perTRP LOS-NLOS-Indicator-r17,

perResource LOS-NLOS-Indicator-r17

} OPTIONAL, -- Need ON

nr-RSCP-r18 INTEGER (0..3599) OPTIONAL, -- Need ON

nr-DL-PRS-RSRP-Result-r18 INTEGER (0..126) OPTIONAL, -- Need ON

nr-DL-PRS-FirstPathRSRP-Result-r18 INTEGER (0..126) OPTIONAL, -- Need ON

nr-PhaseQuality-r18 NR-PhaseQuality-r18 OPTIONAL, -- Need ON

nr-PRU-RSCP-AddSampleMeasurements-r18 SEQUENCE (SIZE (1..nrNumOfSamples-1-r18 )) OF

NR-RSCP-AdditionalMeasurements-r18 OPTIONAL, -- Need ON

nr-PRU-RSRP-AddSampleMeasurements-r18 SEQUENCE (SIZE (1..nrNumOfSamples-1-r18)) OF

INTEGER (0..61) OPTIONAL, -- Need ON

nr-PRU-FirstPathRSRP-ResultDiff-AddSampleMeasurements-r18

SEQUENCE (SIZE (1..nrNumOfSamples-1-r18 )) OF INTEGER (0..61) OPTIONAL, -- Need ON

nr-PRU-RSCP-AdditionalMeasurements-r18

NR-PRU-RSCP-AdditionalMeasurements-r18 OPTIONAL, -- Need ON

...

}

NR-PRU-RSCP-AdditionalMeasurements-r18 ::= SEQUENCE (SIZE (1..3)) OF

NR-PRU-RSCP-AdditionalMeasurementElement-r18

NR-PRU-RSCP-AdditionalMeasurementElement-r18 ::= SEQUENCE {

nr-DL-PRS-ResourceID-r18 NR-DL-PRS-ResourceID-r16 OPTIONAL, -- Need ON

nr-DL-PRS-ResourceSetID-r18 NR-DL-PRS-ResourceSetID-r16 OPTIONAL, -- Need ON

nr-DL-PRS-RSRP-ResultDiff-r18 INTEGER (0..61) OPTIONAL, -- Need ON

nr-DL-PRS-FirstPathRSRP-ResultDiff-r18 INTEGER (0..61) OPTIONAL, -- Need ON

nr-PRU-RSCP-AdditionalMeasurementsList-r18 SEQUENCE (SIZE (1..nrNumOfSamples-r18 )) OF

NR-RSCP-AdditionalMeasurements-r18 OPTIONAL, -- Need ON

nr-PRU-RSRPDiff-AdditionalMeasurementsList-r18 SEQUENCE (SIZE (1..nrNumOfSamples-r18 )) OF INTEGER (0..61) OPTIONAL, -- Need ON

nr-PRU-FirstPathRSRP-ResultDiff-AdditionalMeasurementsList-r18

SEQUENCE (SIZE (1..nrNumOfSamples-r18 )) OF INTEGER (0..61) OPTIONAL, -- Need ON

...

}

-- ASN1STOP

| *NR-PRU-DL-Info* field descriptions |
| --- |
| ***nr-PRU-LocationInfo***  This field provides the location coordinates of the PRU. |
| ***nr-PRU-DL-TDOA-MeasInfo***  This field specifies the list of carrier phase measurement RSCPD together with the other measurement information in DL-TDOA by the PRU. |
| ***nr-PRU-DL-AoD-MeasInfo***  This field specifies the list of other measurement information in DL-AoD by the PRU. |
| ***nr-PRU-RSCP-MeasInfo***  This field specifies the list of carrier phase measurement RSCP measured by the PRU, together with DL-PRS RSRP, and/or DL-PRS RSRPP measurement(s) associated with the RSCP measurements. |

#### – *NR-RTD-Info*

The IE *NR-RTD-Info* is used by the location server to provide time synchronization information between a reference TRP and a list of neighbour TRPs together with integrity information.

-- ASN1START

NR-RTD-Info-r16 ::= SEQUENCE {

referenceTRP-RTD-Info-r16 ReferenceTRP-RTD-Info-r16,

rtd-InfoList-r16 RTD-InfoList-r16,

...

}

ReferenceTRP-RTD-Info-r16 ::= SEQUENCE {

dl-PRS-ID-Ref-r16 INTEGER (0..255),

nr-PhysCellID-Ref-r16 NR-PhysCellID-r16 OPTIONAL, -- Need ON

nr-CellGlobalID-Ref-r16 NCGI-r15 OPTIONAL, -- Need ON

nr-ARFCN-Ref-r16 ARFCN-ValueNR-r15 OPTIONAL, -- Need ON

refTime-r16 CHOICE {

systemFrameNumber-r16 BIT STRING (SIZE (10)),

utc-r16 UTCTime,

...

},

rtd-RefQuality-r16 NR-TimingQuality-r16 OPTIONAL, -- Need ON

...

}

RTD-InfoList-r16 ::= SEQUENCE (SIZE (1..nrMaxFreqLayers-r16)) OF RTD-InfoListPerFreqLayer-r16

RTD-InfoListPerFreqLayer-r16 ::= SEQUENCE (SIZE(1..nrMaxTRPsPerFreq-r16)) OF RTD-InfoElement-r16

RTD-InfoElement-r16 ::= SEQUENCE {

dl-PRS-ID-r16 INTEGER (0..255),

nr-PhysCellID-r16 NR-PhysCellID-r16 OPTIONAL, -- Need ON

nr-CellGlobalID-r16 NCGI-r15 OPTIONAL, -- Need ON

nr-ARFCN-r16 ARFCN-ValueNR-r15 OPTIONAL, -- Need ON

subframeOffset-r16 INTEGER (0..1966079),

rtd-Quality-r16 NR-TimingQuality-r16,

...,

[[

nr-IntegrityRTD-InfoBounds-r18 NR-IntegrityRTD-InfoBounds-r18 OPTIONAL -- Need OR

]]

}

NR-IntegrityRTD-InfoBounds-r18 ::= SEQUENCE {

resolution-r18 ENUMERATED {mdot1, m1, m10, m30, ...},

meanRTD-r18 INTEGER (0..255),

stdDevRTD-r18 INTEGER (0..31),

...

}

-- ASN1STOP

| *NR-RTD-Info* field descriptions |
| --- |
| ***referenceTRP-RTD-Info***  This field defines the reference TRP for the RTD and comprises the following sub-fields:  - ***dl-PRS-ID-Ref***: This field is used along with a DL-PRS Resource Set ID and a DL-PRS Resources ID to uniquely identify a DL-PRS Resource, and is associated to the reference TRP.  - ***nr-PhysCellId-Ref***: This field specifies the physical cell identity of the reference TRP.  - ***nr-CellGlobalId-Ref***: This field specifies the NCGI, the globally unique identity of a cell in NR, of the reference TRP.  - ***nr-ARFCN-Ref***: This field specifies the NR-ARFCN of the TRP's CD-SSB (as defined in TS 38.300 [47]) corresponding to *nr-PhysCellID*.  - ***refTime***: This field specifies the reference time at which the *rtd-InfoList* is valid. The *systemFrameNumber* choice refers to the SFN of the reference TRP.  - ***rtd-RefQuality***: This field specifies the quality of the timing of reference TRP, used to determine the RTD values provided in *rtd-InfoList*. |
| ***dl-PRS-ID***  This field is used along with a DL-PRS Resource Set ID and a DL-PRS Resources ID to uniquely identify a DL-PRS Resource. This ID can be associated with multiple DL-PRS Resource Sets associated with a single TRP for which the *RTD-InfoElement* is applicable. |
| ***nr-PhysCellID***  This field specifies the physical cell identity of the associated TRP for which the *RTD-InfoElement* is applicable, as defined in TS 38.331 [35]. |
| ***nr-CellGlobalID***  This field specifies the NCGI, the globally unique identity of a cell in NR, of the associated TRP for which the *RTD-InfoElement* is applicable, as defined in TS 38.331 [35]. The server should include this field if it considers that it is needed to resolve ambiguity in the TRP indicated by *nr-PhysCellID*. |
| ***nr-ARFCN***  This field specifies the NR-ARFCN of the TRP's CD-SSB (as defined in TS 38.300 [47]) corresponding to *nr-PhysCellID* for which the *RTD-InfoElement* is applicable. |
| ***subframeOffset***  This field specifies the subframe boundary offset at the TRP antenna location between the reference TRP and this neighbour TRP in time units  where Hz and  (TS 38.211 [41]).  The offset is counted from the beginning of a subframe #0 of the reference TRP to the beginning of the closest subsequent subframe of this neighbour TRP.  Scale factor 1 Tc. |
| ***rtd-Quality***  This field specifies the quality of the RTD. |
| ***nr-IntegrityRTD-InfoBounds***  This field specifies an overbounding model that bounds the inter-TRP synchronization error between reference TRP and this TRP. This field comprises the following sub-fields:  ***-*** ***resolution***: The resolution is used in the *meanRTD* and *stdDevRTD*. The enumerated values mdot1, m1, m10, m30 correspond to 0.1, 1, 10, 30 metres, respectively.  - ***meanRTD***: This field specifies the mean inter-TRP synchronization error bound which is the mean value for an overbounding model that bounds the inter-TRP synchronization error. The bound is *meanRTD* + K \* *stdDevRTD* and shall be so that the probability of it to be exceeded shall be lower than IRallocation for ir-Minimum < IRallocation < ir-Maximum, where K = normInv(IRallocation / 2) and ir-Minimum, ir-Maximum as provided in IE *NR-IntegrityServiceParameters*. This IRallocation is a fraction of the Target Integrity Risk that represents the integrity risk budget available.  - ***stdDevRTD***: This field specifies the standard deviation inter-TRP synchronization error bound which is the standard deviation for an overbounding model that bounds the inter-TRP synchronization error. |

#### – *NR-SelectedDL-PRS-IndexList*

The IE *NR-SelectedDL-PRS-IndexList* is used by the location server to provide the selected DL-PRS Resource of *nr-DL-PRS-AssistanceDataList* to the target device.

In the case of assistance data for multiple NR positioning methods are provided, the IE *NR-DL-PRS-AssistanceData* shall be present in only one of *NR-Multi-RTT-ProvideAssistanceData*, *NR-DL-AoD-ProvideAssistanceData*, *NR-DL-TDOA-ProvideAssistanceData*, or *NR-AI-ML-PositioningProvideAssistanceData*.

Editor's Note: It is FFS whether DL-PRS assistance data are applicable to AI/ML positioning.

-- ASN1START

NR-SelectedDL-PRS-IndexList-r16 ::= SEQUENCE (SIZE (1..nrMaxFreqLayers-r16)) OF

NR-SelectedDL-PRS-PerFreq-r16

NR-SelectedDL-PRS-PerFreq-r16 ::= SEQUENCE {

nr-SelectedDL-PRS-FrequencyLayerIndex-r16 INTEGER (0..nrMaxFreqLayers-1-r16),

nr-SelectedDL-PRS-IndexListPerFreq-r16 SEQUENCE (SIZE (1..nrMaxTRPsPerFreq-r16)) OF

NR-SelectedDL-PRS-IndexPerTRP-r16

OPTIONAL, --Need OP

...

}

NR-SelectedDL-PRS-IndexPerTRP-r16 ::= SEQUENCE {

nr-SelectedTRP-Index-r16 INTEGER (0..nrMaxTRPsPerFreq-1-r16),

dl-SelectedPRS-ResourceSetIndexList-r16 SEQUENCE (SIZE (1..nrMaxSetsPerTrpPerFreqLayer-r16))

OF DL-SelectedPRS-ResourceSetIndex-r16

OPTIONAL, --Need OP

...

}

DL-SelectedPRS-ResourceSetIndex-r16 ::= SEQUENCE {

nr-DL-SelectedPRS-ResourceSetIndex-r16 INTEGER (0..nrMaxSetsPerTrpPerFreqLayer-1-r16),

dl-SelectedPRS-ResourceIndexList-r16 SEQUENCE (SIZE (1..nrMaxResourcesPerSet-r16)) OF

DL-SelectedPRS-ResourceIndex-r16

OPTIONAL --Need OP

}

DL-SelectedPRS-ResourceIndex-r16 ::= SEQUENCE {

nr-DL-SelectedPRS-ResourceIdIndex-r16 INTEGER (0..nrMaxNumDL-PRS-ResourcesPerSet-1-r16),

...

}

-- ASN1STOP

| *NR-SelectedDL-PRS-IndexList* field descriptions |
| --- |
| ***nr-SelectedDL-PRS-FrequencyLayerIndex***  This field indicates the frequency layer provided in IE *NR-DL-PRS-AssistanceData*. Value 0 corresponds to the first frequency layer provided in *nr-DL-PRS-AssistanceDataList* in IE *NR-DL-PRS-AssistanceData*, value 1 to the second frequency layer in *nr-DL-PRS-AssistanceDataList*, and so on. |
| ***nr-SelectedDL-PRS-IndexListPerFreq***  This field provides the list of addressed TRPs of the selected frequency layer. If this field is absent, all DL-PRS Resources of all TRPs of the indicated frequency layer are addressed. |
| ***nr-SelectedTRP-Index***  This field indicates the addressed TRP of the selected frequency layer. Value 0 corresponds to the first entry in *nr-DL-PRS-AssistanceDataPerFreq* provided in IE *NR-DL-PRS-AssistanceData*, value 1 corresponds to the second entry in *nr-DL-PRS-AssistanceDataPerFreq*, and so on. |
| ***dl-SelectedPRS-ResourceSetIndexList***  This field provides the list of addressed DL-PRS Resource Sets of the selected TRPs of the selected frequency layer. If this field is absent, all DL-PRS Resource Sets and Resources of the indicated TRP are addressed. |
| ***nr-DL-SelectedPRS-ResourceSetIndex***  This field indicates the addressed DL-PRS Resource Set of the selected TRP of the selected frequency layer. Value 0 corresponds to the first entry in *nr-DL-PRS-ResourceSetList* in IE *NR-DL-PRS-Info* provided in IE *NR-DL-PRS-AssistanceData*. Value 1 corresponds to the second entry in the *nr-DL-PRS-ResourceSetList* in IE *NR-DL-PRS-Info*. |
| ***dl-SelectedPRS-ResourceIndexList***  This field provides the list of addressed DL-PRS Resources of the selected DL-PRS Resource Set of the selected TRP of the selected frequency layer. If this field is absent, all DL-PRS Resources of the indicated DL-PRS Resource Set are addressed. |
| ***nr-dl-SelectedPRS-ResourceIdIndex***  This field indicates the addressed DL-PRS Resource of the selected DL-PRS Resource Set of the TRP of the selected frequency layer. Value 0 corresponds to the first entry in *dl-PRS-ResourceList* in IE *NR-DL-PRS-Info* provided in IE *NR-DL-PRS-AssistanceData*. Value 1 corresponds to the second entry in the *dl-PRS-ResourceList* in IE *NR-DL-PRS-Info*, and so on. |

#### *– NR-SSB-Config*

The IE *NR-SSB-Config* defines SSB configuration.

-- ASN1START

NR-SSB-Config-r16 ::= SEQUENCE {

nr-PhysCellID-r16 NR-PhysCellID-r16,

nr-ARFCN-r16 ARFCN-ValueNR-r15,

ss-PBCH-BlockPower-r16 INTEGER (-60..50),

halfFrameIndex-r16 INTEGER (0..1),

ssb-periodicity-r16 ENUMERATED { ms5, ms10, ms20, ms40, ms80, ms160, ...},

ssb-PositionsInBurst-r16 CHOICE {

shortBitmap-r16 BIT STRING (SIZE (4)),

mediumBitmap-r16 BIT STRING (SIZE (8)),

longBitmap-r16 BIT STRING (SIZE (64))

} OPTIONAL, --Need OR

ssb-SubcarrierSpacing-r16 ENUMERATED {kHz15, kHz30, kHz60, kHz120, kHz240, ...},

sfn-SSB-Offset-r16 INTEGER (0..15),

...

}

-- ASN1STOP

| *NR-SSB-Config* field descriptions |
| --- |
| ***nr-ARFCN***  This field specifies the ARFCN of the first RE of SSB's RB#10. |
| ***ss-PBCH-BlockPower***  Average EPRE of the resources elements that carry secondary synchronization signals in dBm that the NW used for SSB transmission, see TS 38.213 [48], clause 7. |
| ***halfFrameIndex***  Indicates the 5 msec offset of the SSB within a 10 msec system frame. |
| ***ssb-periodicity***  The SSB periodicity in ms for the rate matching purpose. |
| ***ssb-PositionsInBurst***  Indicates the time domain positions of the transmitted SS-blocks in a half frame with SS/PBCH blocks as defined in TS 38.213 [48], clause 4.1. The first/leftmost bit corresponds to SS/PBCH block index 0, the second bit corresponds to SS/PBCH block index 1, and so on. Value 0 in the bitmap indicates that the corresponding SS/PBCH block is not transmitted while value 1 indicates that the corresponding SS/PBCH block is transmitted. |
| ***ssb-SubcarrierSpacing***  Subcarrier spacing of SSB. Only the values 15 kHz or 30 kHz (FR1), and 120 kHz or 240 kHz (FR2) are applicable. |
| ***sfn-SSB-Offset***  Indicates the 10 msec system frame offset of the SSB within the SSB periodicity. Value 0 indicates that the SSB is transmitted in the first system frame; 1 indicates that the SSB is transmitted in the second system frame and so on. This field shall be configured according to the field *ssb-Periodicity* and the indicated system frame shall not exceed the configured SSB periodicity. |

#### *– NR-TimeStamp*

The IE *NR-TimeStamp* defines the UE measurement associated time stamp.

-- ASN1START

NR-TimeStamp-r16 ::= SEQUENCE {

dl-PRS-ID-r16 INTEGER (0..255),

nr-PhysCellID-r16 NR-PhysCellID-r16 OPTIONAL, -- Need ON

nr-CellGlobalID-r16 NCGI-r15 OPTIONAL, -- Need ON

nr-ARFCN-r16 ARFCN-ValueNR-r15 OPTIONAL, -- Need ON

nr-SFN-r16 INTEGER (0..1023),

nr-Slot-r16 CHOICE {

scs15-r16 INTEGER (0..9),

scs30-r16 INTEGER (0..19),

scs60-r16 INTEGER (0..39),

scs120-r16 INTEGER (0..79)

},

...,

[[

nr-Symbol-r18 INTEGER (0..13) OPTIONAL -- Need ON

]]

}

-- ASN1STOP

| *NR-TimeStamp* field descriptions |
| --- |
| ***dl-PRS-ID***  This field specifies the DL-PRS ID of the TRP for which the *nr-SFN* is applicable. |
| ***nr-PhysCellID***  This field specifies the physical cell identity of the associated TRP, as defined in TS 38.331 [35]. |
| ***nr-CellGlobalID***  This field specifies the NCGI, the globally unique identity of a cell in NR, of the associated TRP, as defined in TS 38.331 [35]. |
| ***nr-ARFCN***  This field specifies the ARFCN of the TRP's CD-SSB (as defined in TS 38.300 [47]) corresponding to *nr-PhysCellID* associated with the *dl-PRS-ID*. |
| ***nr-SFN***  This field specifies the NR system frame number for the time stamp. |
| ***nr-Slot***  This field specifies the NR slot number within the NR system frame number indicated by *nr-SFN* for the time stamp. |
| ***nr-Symbol***  This field specifies the NR symbol index within the NR slot number indicated by *nr-Slot* for the time stamp for RSCP/RSCPD measurement. |

#### *– NR-TimingQuality*

The IE *NR-TimingQuality* defines the quality of a timing value (e.g., of a TOA measurement).

-- ASN1START

NR-TimingQuality-r16 ::= SEQUENCE {

timingQualityValue-r16 INTEGER (0..31),

timingQualityResolution-r16 ENUMERATED {mdot1, m1, m10, m30, ...},

...

}

-- ASN1STOP

| *NR-TimingQuality* field descriptions |
| --- |
| ***timingQualityValue***  This field provides an estimate of uncertainty of the timing value for which the IE *NR-TimingQuality* is provided in units of metres. |
| ***timingQualityResolution***  This field provides the resolution used in the *timingQualityValue* field. Enumerated values *mdot1*, *m1*, *m10*, *m30* correspond to 0.1, 1, 10, 30 metres, respectively. |

#### – *NR-TRP-BeamAntennaInfo*

The IE *NR-TRP-BeamAntennaInfo* is used by the location server to provide beam antenna information of the TRP together with integrity information.

-- ASN1START

NR-TRP-BeamAntennaInfo-r17 ::= SEQUENCE (SIZE (1..nrMaxFreqLayers-r16)) OF

NR-TRP-BeamAntennaInfoPerFreqLayer-r17

NR-TRP-BeamAntennaInfoPerFreqLayer-r17 ::= SEQUENCE (SIZE (1..nrMaxTRPsPerFreq-r16)) OF

NR-TRP-BeamAntennaInfoPerTRP-r17

NR-TRP-BeamAntennaInfoPerTRP-r17 ::= SEQUENCE {

dl-PRS-ID-r17 INTEGER (0..255),

nr-PhysCellID-r17 NR-PhysCellID-r16 OPTIONAL, -- Need ON

nr-CellGlobalID-r17 NCGI-r15 OPTIONAL, -- Need ON

nr-ARFCN-r17 ARFCN-ValueNR-r15 OPTIONAL, -- Need ON

associated-DL-PRS-ID-r17 INTEGER (0..255) OPTIONAL, -- Need OP

lcs-GCS-TranslationParameter-r17 LCS-GCS-TranslationParameter-r16 OPTIONAL, -- Need OP

nr-TRP-BeamAntennaAngles-r17 NR-TRP-BeamAntennaAngles-r17 OPTIONAL, -- Need OP

...

}

NR-TRP-BeamAntennaAngles-r17 ::= SEQUENCE (SIZE(1..3600)) OF

NR-TRP-BeamAntennaInfoAzimuthElevation-r17

NR-TRP-BeamAntennaInfoAzimuthElevation-r17 ::= SEQUENCE {

azimuth-r17 INTEGER (0..359) OPTIONAL, -- Cond Az

azimuth-fine-r17 INTEGER (0..9) OPTIONAL, -- Cond AzOpt

elevationList-r17 SEQUENCE (SIZE(1..1801)) OF ElevationElement-R17,

...

}

ElevationElement-R17 ::= SEQUENCE {

elevation-r17 INTEGER (0..180) OPTIONAL, -- Cond El

elevation-fine-r17 INTEGER (0..9) OPTIONAL, -- Cond ElOpt

beamPowerList-r17 SEQUENCE (SIZE (2..maxNumResourcesPerAngle-r17)) OF

BeamPowerElement-r17,

...

}

BeamPowerElement-r17 ::= SEQUENCE {

nr-dl-prs-ResourceSetID-r17 NR-DL-PRS-ResourceSetID-r16 OPTIONAL, -- Need OP

nr-dl-prs-ResourceID-r17 NR-DL-PRS-ResourceID-r16,

nr-dl-prs-RelativePower-r17 INTEGER (0..30),

nr-dl-prs-RelativePowerFine-r17 INTEGER (0..9) OPTIONAL, -- Need ON

...,

[[

nr-IntegrityBeamPowerBounds-r18 NR-IntegrityBeamPowerBounds-r18 OPTIONAL -- Need OP

]]

}

NR-IntegrityBeamPowerBounds-r18 ::= SEQUENCE {

meanBeamPower-r18 INTEGER (0..127),

stdDevBeamPower-r18 INTEGER (0..127),

...

}

-- ASN1STOP

| Conditional presence | Explanation |
| --- | --- |
| *Az* | The field is mandatory present if the field *elevation* is absent; otherwise it is optionally present, need ON. |
| *AzOpt* | The field is optionally present, need ON, when *azimuth* is present; otherwise it is not present. |
| *El* | The field is mandatory present if the field *azimuth* is absent; otherwise it is optionally present, need ON. |
| *ElOpt* | The field is optionally present, need ON, when *elevation* is present; otherwise it is not present. |

| *NR-TRP-BeamAntennaInfo* field descriptions |
| --- |
| ***dl-PRS-ID***  This field specifies the DL-PRS ID of the TRP for which the Beam Antenna Information is provided. |
| ***nr-PhysCellID***  This field specifies the physical Cell-ID of the TRP for which the Beam Antenna Information is provided, as defined in TS 38.331 [35]. |
| ***nr-CellGlobalID***  This field specifies the NCGI, the globally unique identity of a cell in NR, of the TRP for which the Beam Antenna Information is provided, as defined in TS 38.331 [35]. |
| ***nr-ARFCN***  This field specifies the NR-ARFCN of the TRP's CD-SSB (as defined in TS 38.300 [47]) corresponding to *nr-PhysCellID*. |
| ***associated-DL-PRS-ID***  This field specifies the *dl-PRS-ID* of the associated TRP from which the beam antenna information is obtained. See the field descriptions for *nr-TRP-BeamAntennaAngles* and *lcs-GCS-TranslationParameter*. |
| ***lcs-GCS-TranslationParameter***  This field provides the angles α (bearing angle), β (downtilt angle) and γ (slant angle) for the translation of a Local Coordinate System (LCS) to a Global Coordinate System (GCS) as defined in TR 38.901 [44]. If this field and the *associated-DL-PRS-ID* field are both absent, the *azimuth* and *elevation* are provided in a GCS. If this field is absent and the *associated-DL-PRS-ID* field is present, then the *lcs-GCS-TranslationParameter* for this TRP is obtained from the *lcs-GCS-TranslationParameter* of the associated TRP. |
| ***nr-TRP-BeamAntennaAngles***  This field provides the relative power between DL-PRS Resources per angle per TRP. If this field is absent and the field *associated-DL-PRS-ID* is present, the *nr-TRP-BeamAntennaAngles* for this TRP are obtained from the *nr-TRP-BeamAntennaAngles* of the associated TRP. |
| ***azimuth***  This field specifies the azimuth angle for which the relative power between DL-PRS Resources is provided.  For a Global Coordinate System (GCS), the azimuth angle is measured counter-clockwise from geographical North.  For a Local Coordinate System (LCS), the azimuth angle is measured counter-clockwise from the x-axis of the LCS.  Scale factor 1 degree; range 0 to 359 degrees. |
| ***azimuth-fine***  This field provides finer granularity for the *azimuth*.  The total azimuth angle is given by *azimuth* + *azimuth-fine.*  Scale factor 0.1 degrees; range 0 to 0.9 degrees. |
| ***elevation***  This field specifies the elevation angle for which the relative power between DL-PRS Resources is provided for the given *azimuth*.  For a Global Coordinate System (GCS), the elevation angle is measured relative to zenith and positive to the horizontal direction (elevation 0 deg. points to zenith, 90 deg to the horizon).  For a Local Coordinate System (LCS), the elevation angle is measured relative to the z-axis of the LCS (elevation 0 deg. points to the z-axis, 90 deg to the x-y plane).  Scale factor 1 degree; range 0 to 180 degrees. |
| ***elevation-fine***  This field provides finer granularity for the *elevation*.  The total elevation angle is given by *elevation* + *elevation-fine.*  Scale factor 0.1 degrees; range 0 to 0.9 degrees. |
| ***beamPowerList***  This field provides the relative power between DL-PRS Resources for the angle given by *azimuth* and *elevation*.  The first *BeamPowerElement* in this list provides the peak power for this angle and is defined as 0dB power; i.e., the first value is set to '0' by the location server. All the remaining *BeamPowerElement*'s in this list provide the relative DL-PRS Resource power relative to this first element in the list. |
| ***nr-dl-prs-ResourceSetID***  This field specifies the DL-PRS Resource Set ID of the DL-PRS Resource for which the *nr-dl-prs-RelativePower* is provided. If this field is absent, the DL-PRS Resource Set ID for this instance of the *beamPowerList* is the same as the DL-PRS Resource Set ID of the previous instance in the *beamPowerList*. This field shall be included at least in the first instance of the *beamPowerList*. |
| ***nr-dl-prs-ResourceID***  This field specifies the DL-PRS Resource for which the *nr-dl-prs-RelativePower* is provided. |
| ***nr-dl-prs-RelativePower***  Except for the first element in *beamPowerList*, this field provides the relative power of the DL-PRS Resource, relative to the first element in the *beamPowerList*.  For the first element in *beamPowerList*, this field provides the peak power for this angle normalised to 0 dB.  Scale factor 1 dB; range 0..-30 dB. |
| ***nr-dl-prs-RelativePowerFine***  This field provides finer granularity for the *nr-dl-prs-RelativePower*.  The total relative power of the DL-PRS Resource is given by *nr-dl-prs-RelativePower* + *nr-dl-prs-RelativePowerFine.*  Scale factor -0.1 dB; range 0 to -0.9 dB.  NOTE: For the first element in *beamPowerList*, this field is not needed. |
| ***nr-IntegrityBeamPowerBounds***  This field specifies the mean and the Standard Deviation beam power error bound for an overbounding model that bounds the beam power error. If this field is absent, the *nr-IntegrityBeamInfoBounds* for this instance of the *beamPowerList* is the same as *nr-IntegrityBeamInfoBounds* of the previous instance in the *beamPowerList*. If integrity bounds are provided, this field shall be included at least in the first instance of the *beamPowerList*.  - ***meanBeamPower***: This field specifies the Mean Beam Power Error bound which is the mean value for an overbounding model that bounds the beam power error of the DL-PRS Resources. The bound is *meanBeamPower* + K \* *stdDevBeamPower* and shall be so that the probability of it to be exceeded shall be lower than IRallocation for *ir-Minimum* < IRallocation < *ir-Maximum*, where K = normInv(IRallocation / 2) and *ir-Minimum*, *irMaximum* as provided in IE *NR-IntegrityServiceParameters*. This IRallocation is a fraction of the Target Integrity Risk that represents the integrity risk budget available.  Scale factor 0.1 dB; range 0-12.7 dB.  - ***stdDevBeamPower***: This field specifies the Standard Deviation Beam Power Error bound which is the standard deviation for an overbounding model that bounds the beam power error of the DL-PRS Resources.  Scale factor 0.1 degrees; range 0-12.7 dB. |

#### *–* *NR-TRP-LocationInfo*

The IE *NR-TRP-LocationInfo* is used by the location server to provide the coordinates of TRPs and coordinates of the antenna reference points for a set of TRPs together with integrity information. For each TRP, the ARP location can be provided for each associated DL-PRS Resource ID per DL-PRS Resource Set.

-- ASN1START

NR-TRP-LocationInfo-r16 ::= SEQUENCE (SIZE (1..nrMaxFreqLayers-r16)) OF

NR-TRP-LocationInfoPerFreqLayer-r16

NR-TRP-LocationInfoPerFreqLayer-r16 ::= SEQUENCE {

referencePoint-r16 ReferencePoint-r16 OPTIONAL, -- Cond NotSameAsPrev

trp-LocationInfoList-r16 SEQUENCE (SIZE (1..nrMaxTRPsPerFreq-r16)) OF

TRP-LocationInfoElement-r16,

...

}

TRP-LocationInfoElement-r16 ::= SEQUENCE {

dl-PRS-ID-r16 INTEGER (0..255),

nr-PhysCellID-r16 NR-PhysCellID-r16 OPTIONAL, -- Need ON

nr-CellGlobalID-r16 NCGI-r15 OPTIONAL, -- Need ON

nr-ARFCN-r16 ARFCN-ValueNR-r15 OPTIONAL, -- Need ON

associated-DL-PRS-ID-r16 INTEGER (0..255) OPTIONAL, -- Need OP

trp-Location-r16 RelativeLocation-r16 OPTIONAL, -- Need OP

trp-DL-PRS-ResourceSets-r16 SEQUENCE (SIZE(1..nrMaxSetsPerTrpPerFreqLayer-r16)) OF

DL-PRS-ResourceSets-TRP-Element-r16 OPTIONAL, -- Need OP

...,

[[

trp-LocationCartesian-r18 RelativeCartesianLocation-r18 OPTIONAL, -- Need OP

nr-IntegrityTRP-LocationBounds-r18

NR-IntegrityLocationBounds-r18 OPTIONAL -- Need OR

]]

}

DL-PRS-ResourceSets-TRP-Element-r16 ::= SEQUENCE {

dl-PRS-ResourceSetARP-r16 RelativeLocation-r16 OPTIONAL, -- Need OP

dl-PRS-Resource-ARP-List-r16 SEQUENCE (SIZE(1..nrMaxResourcesPerSet-r16)) OF

DL-PRS-Resource-ARP-Element-r16 OPTIONAL, -- Need OP

...,

[[

dl-PRS-ResourceSetARP-Cartesian-r18 RelativeCartesianLocation-r18 OPTIONAL, -- Need OP

nr-IntegrityDL-PRS-ResourceSetARP-LocationBounds-r18

NR-IntegrityLocationBounds-r18 OPTIONAL -- Need OR

]]

}

DL-PRS-Resource-ARP-Element-r16 ::= SEQUENCE {

dl-PRS-Resource-ARP-location-r16 RelativeLocation-r16 OPTIONAL, -- Need OP

...,

[[

dl-PRS-Resource-ARP-locationCartesian-r18

RelativeCartesianLocation-r18 OPTIONAL, -- Need OP

nr-IntegrityDL-PRS-ResourceARP-LocationBounds-r18

NR-IntegrityLocationBounds-r18 OPTIONAL -- Need OR

]]

}

NR-IntegrityLocationBounds-r18 ::= SEQUENCE {

units-r18 ENUMERATED {mm, cm, m, ...},

meanLocationErrorBound-r18 SEQUENCE {

horizontal-r18 INTEGER (0..255),

vertical-r18 INTEGER (0..255)

},

stdDevLocationErrorBound-r18 SEQUENCE {

horizontal-r18 INTEGER (0..255),

vertical-r18 INTEGER (0..255)

},

...

}

-- ASN1STOP

| Conditional presence | Explanation |
| --- | --- |
| *NotSameAsPrev* | The field is mandatory present in the first entry of the *NR-TRP-LocationInfoPerFreqLayer* in the *nr-TRP-LocationInfo* list; otherwise it is optionally present, need OP. |

| *NR-TRP-LocationInfo* field descriptions |
| --- |
| ***referencePoint***  This field specifies the reference point used to define the location of TRPs provided in the *trp-LocationInfoList*. If this field is absent, the reference point is the same as in the previous entry of the *NR-TRP-LocationInfoPerFreqLayer* in the *NR-TRP-LocationInfo* list. |
| ***trp-LocationInfoList***  This field provides the antenna reference point locations of the DL-PRS Resources for the TRPs together with integrity information and comprises the following sub-fields:  - ***dl-PRS-ID***: This field is used along with a DL-PRS Resource Set ID and a DL-PRS Resource ID to uniquely identify a DL-PRS Resource, and is associated to a single TRP.  - ***nr-PhysCellID***: This field specifies the physical cell identity of the associated TRP.  - ***nr-CellGlobalID***: This field specifies the NCGI, the globally unique identity of a cell in NR, of the associated TRP.  - ***nr-ARFCN***: This field specifies the NR-ARFCN of the TRP's CD-SSB (as defined in TS 38.300 [47]) corresponding to *nr-PhysCellID*.  - ***associated-DL-PRS-ID***: This field, if present, specifies the *dl-PRS-ID* of the associated TRP from which the *trp-location* or *trp-LocationCartesian* information is adopted. If the field is present, the field *trp-Location* and *trp-LocationCartesian* shall be absent.  - ***trp-Location, trp-LocationCartesian***: This field provides the location of the TRP relative to the *referencePoint* location either in geodetic coordinates (*trp-Location*)or local Cartesian coordinates (*trp-LocationCartesian*). If none of *trp-Location*, *trp-LocationCartesian* is present, the TRP location coincides with the *referencePoint* location, unless the field *associated-dl-PRS-ID*is present, in which case the *trp-Location* or *trp-LocationCartesian* is adopted from the associated TRP indicated by *associated-dl-PRS-ID*.  - ***nr-IntegrityTRP-LocationBounds***: This field provides the mean and standard deviation TRP location error bound which is the mean value and the standard deviation of an overbounding model that bounds the TRP location error. This field comprises the following sub-fields:  - ***units***: This field specifies the units (scale factor) for the *meanLocationErrorBound* and s*tdDevLocationErrorBound*. Enumerated values mm, cm, and m correspond to 10-3 metre, 10-2 metre, and 1 metre, respectively.  - ***meanLocationErrorBound***: This field specifies the mean TRP Location Error bound in horizontal and vertical direction, which are the mean values for a set of two overbounding models that bound the TRP location error in horizontal and vertical directions.  Scale factor is 1 with units provided in *units* field.  - ***stdDevLocationErrorBound***: This field specifies the standard deviation TRP Location Error bound in horizontal and vertical direction, which are the standard deviation values for a set of two overbounding models that bound the TRP location error in horizontal and vertical directions.  Scale factor is 1 with units provided in *units* field.  - ***trp-DL-PRS-ResourceSets***: This field provides the antenna reference point location(s) of the DL-PRS Resource Set(s) associated with this TRP together with integrity information. If this field is absent, the antenna reference point location(s) of the DL-PRS Resource Set(s) coincides with the *trp-Location/trp-LocationCartesian* location. This field comprises the following sub-fields:  - ***dl-PRS-ResourceSetARP, dl-PRS-ResourceSetARP-Cartesian***: This field provides the antenna reference point location of the DL-PRS Resource Set relative to the *trp-Location* or *trp-LocationCartesian* location. If none of *dl-PRS-ResourceSetARP*, *dl-PRS-ResourceSetARP-Cartesian* is present, the antenna reference point location of this DL-PRS Resource Set coincides with the *trp-Location* or *trp-LocationCartesian* location.  - ***nr-IntegrityDL-PRS-ResourceSetARP-LocationBounds***: This field provides the mean and the standard deviation ARP of the location error bound of the DL-PRS Resource Set of an overbounding model that bounds the antenna reference point location error of the DL-PRS Resource Set. This field comprises the sub-fields *units***,** *meanLocationErrorBound,* and *stdDevLocationErrorBound****,*** as described under *nr-IntegrityTRP-LocationBounds*.  - ***dl-PRS-Resource-ARP-List***: This field provides the antenna reference point location(s) of the DL-PRS Resource(s) associated with this Resource Set of the TRP together with integrity information. If this field is absent, the antenna reference point location(s) of the DL-PRS Resources coincides with the *dl-PRS-ResourceSetARP* location or *dl-PRS-ResourceSetARP-Cartesian*. This field comprises the following sub-fields:  - ***dl-PRS-Resource-ARP-location, dl-PRS-Resource-ARP-locationCartesian***: This field provides the antenna reference point location of the DL-PRS Resource associated with the DL-PRS Resource Set of the TRP relative to the *dl-PRS-ResourceSetARP/dl-PRS-ResourceSetARP-Cartesian* location. If none of *dl-PRS-Resource-ARP-location*, *dl-PRS-Resource-ARP-locationCartesian* is present, the antenna reference point location of this DL-PRS Resource coincides with the *dl-PRS-ResourceSetARP* location or *dl-PRS-Resource-ARP-locationCartesian*.  - ***nr-IntegrityDL-PRS-ResourceARP-LocationBounds***: This field provides the mean and the standard deviation ARP of the location error bound of the DL-PRS Resources of an overbounding model that bounds the antenna reference point location error of the DL-PRS Resource. This field comprises the sub-fields *units***,** *meanLocationErrorBound,* and *stdDevLocationErrorBound****,*** as described under *nr-IntegrityTRP-LocationBounds*. |

NOTE 5: The locations may be provided in either geodetic coordinates (*RelativeLocation*) or local Cartesian coordinates (*RelativeCartesianLocation*), but not both. Local Cartesian coordinates are provided with respect to the *horizAxesOrientation* of the local origin defined by the *referencePoint* field.

#### *– NR-UE-TEG-Capability*

The IE *NR-UE-TEG-Capability* defines the TEG capability of the target device.

-- ASN1START

NR-UE-TEG-Capability-r17 ::= SEQUENCE {

nr-UE-TEG-ID-CapabilityBandList-r17 SEQUENCE (SIZE (1..nrMaxBands-r16)) OF

NR-UE-TEG-ID-CapabilityPerBand-r17 OPTIONAL,

...

}

NR-UE-TEG-ID-CapabilityPerBand-r17 ::= SEQUENCE {

freqBandIndicatorNR-r17 FreqBandIndicatorNR-r16,

nr-UE-RxTEG-ID-MaxSupport-r17 ENUMERATED {n1, n2, n3, n4, n6, n8} OPTIONAL,

nr-UE-TxTEG-ID-MaxSupport-r17 ENUMERATED {n1, n2, n3, n4, n6, n8} OPTIONAL,

nr-UE-RxTxTEG-ID-MaxSupport-r17 ENUMERATED {n1, n2, n4, n6, n8, n12, n16,

n24, n32, n36, n48, n64} OPTIONAL,

measureSameDL-PRS-ResourceWithDifferentRxTEGs-r17

ENUMERATED {n2, n3, n4, n6, n8} OPTIONAL,

measureSameDL-PRS-ResourceWithDifferentRxTEGsSimul-r17

ENUMERATED {n1, n2, n3, n4, n6, n8} OPTIONAL,

...

}

-- ASN1STOP

| *NR-UE-TEG-Capability* field descriptions |
| --- |
| ***nr-UE-RxTEG-ID-MaxSupport***  Indicates the maximum number of UE-RxTEGs, which is supported and reported by the UE. This field is applicable for UE assisted DL-TDOA and Multi-RTT positioning. The UE can include this field only if the UE supports *prs-ProcessingCapabilityBandList* and any of *maxNrOfDL-PRS-ResourceSetPerTrpPerFrequencyLayer*, *maxNrOfTRP-AcrossFreqs*, *maxNrOfPosLayer*, *maxNrOfDL-PRS-ResourcesPerResourceSet* and *maxNrOfDL-PRS-ResourcesPerPositioningFrequencylayer*. Otherwise, the UE does not include this field.  NOTE 1: A single value is reported when both Multi-RTT and DL-TDOA are supported. |
| ***nr-UE-TxTEG-ID-MaxSupport***  Indicates the maximum number of UE-TxTEGs, which is supported and reported by the UE. This field is applicable for Multi-RTT and UL-TDOA positioning. For UL-TDOA, the UE can include this field only if the UE supports *supportedSRS-PosResources* defined in TS 38.331 [35]. For Multi-RTT, the UE can include this field only if the UE supports *maxNrOfDL-PRS-ResourcesPerResourceSet,* *maxNrOfDL-PRS-ResourcesPerPositioningFrequencylayer* and *supportedSRS-PosResources* defined in TS 38.331 [35]. Otherwise, the UE does not include this field. |
| ***nr-UE-RxTxTEG-ID-MaxSupport***  Indicates the maximum number of UE-RxTxTEGs, which is supported and reported by the UE. This field is applicable for Multi-RTT positioning. The UE can include this field only if the UE supports *maxNrOfDL-PRS-ResourcesPerResourceSet,* *maxNrOfDL-PRS-ResourcesPerPositioningFrequencylayer* and *supportedSRS-PosResources* defined in TS 38.331 [35]. Otherwise, the UE does not include this field. |
| ***measureSameDL-PRS-ResourceWithDifferentRxTEGs***  Indicates the maximum number of different UE-RxTEGs that a UE can support to measure the same DL-PRS Resource of a TRP. This field is applicable for UE assisted DL-TDOA and Multi-RTT positioning. The UE can include this field only if the UE supports *nr-UE-RxTEG-ID-MaxSupport*. Otherwise, the UE does not include this field.  NOTE 2: If the UE supports *nr-UE-RxTxTEG-ID-MaxSupport* and *measureSameDL-PRS-ResourceWithDifferentRxTEGs*, the enumerated value of this field also corresponds to the maximum number of different UE-RxTx TEGs for measuring the same DL-PRS Resource of a TRP with the same UE Tx TEG. |
| ***measureSameDL-PRS-ResourceWithDifferentRxTEGsSimul***  Indicates the maximum number of UE Rx TEGs for measuring the same DL-PRS Resource simultaneously. This field is applicable for UE assisted DL-TDOA and Multi-RTT positioning. The UE can include this field only if the UE supports *measureSameDL-PRS-ResourceWithDifferentRxTEGs*. Otherwise, the UE does not include this field.  NOTE 3: If the UE supports *nr-UE-RxTxTEG-ID-MaxSupport* and *measureSameDL-PRS-ResourceWithDifferentRxTEGs* and *measureSameDL-PRS-ResourceWithDifferentRxTEGsSimul*, the enumerated value of this field also corresponds to the maximum number of different UE-RxTx TEGs for measuring the same DL-PRS Resource simultaneously with the same UE Tx TEG. |

#### *– NR-UL-SRS-Capability*

The IE *NR-UL-SRS-Capability* defines the UE uplink SRS capability.

-- ASN1START

NR-UL-SRS-Capability-r16 ::= SEQUENCE {

srs-CapabilityBandList-r16 SEQUENCE (SIZE (1..nrMaxBands-r16)) OF

SRS-CapabilityPerBand-r16,

srs-PosResourceConfigCA-BandList-r16 SEQUENCE (SIZE (1..nrMaxConfiguredBands-r16)) OF

SRS-PosResourcesPerBand-r16 OPTIONAL,

maxNumberSRS-PosPathLossEstimateAllServingCells-r16

ENUMERATED {n1, n4, n8, n16} OPTIONAL,

maxNumberSRS-PosSpatialRelationsAllServingCells-r16

ENUMERATED {n0, n1, n2, n4, n8, n16} OPTIONAL,

...

}

SRS-CapabilityPerBand-r16 ::= SEQUENCE {

freqBandIndicatorNR-r16 FreqBandIndicatorNR-r16,

olpc-SRS-Pos-r16 OLPC-SRS-Pos-r16 OPTIONAL,

spatialRelationsSRS-Pos-r16 SpatialRelationsSRS-Pos-r16 OPTIONAL,

...,

[[

posSRS-RRC-Inactive-InInitialUL-BWP-r17 PosSRS-RRC-Inactive-InInitialUL-BWP-r17 OPTIONAL,

posSRS-RRC-Inactive-OutsideInitialUL-BWP-r17

PosSRS-RRC-Inactive-OutsideInitialUL-BWP-r17

OPTIONAL,

olpc-SRS-PosRRC-Inactive-r17 OLPC-SRS-Pos-r16 OPTIONAL,

spatialRelationsSRS-PosRRC-Inactive-r17 SpatialRelationsSRS-Pos-r16 OPTIONAL

]],

[[

posSRS-SP-RRC-Inactive-InInitialUL-BWP-r17 PosSRS-SP-RRC-Inactive-InInitialUL-BWP-r17

OPTIONAL

]],

[[

posSRS-Preconfigured-RRC-InactiveInitialUL-BWP-r18 ENUMERATED {supported} OPTIONAL,

posSRS-Preconfigured-RRC-InactiveOutsideInitialUL-BWP-r18 ENUMERATED {supported} OPTIONAL,

posSRS-ValidityAreaRRC-InactiveInitialUL-BWP-r18 ENUMERATED {supported} OPTIONAL,

posSRS-ValidityAreaRRC-InactiveOutsideInitialUL-BWP-r18 ENUMERATED {supported} OPTIONAL,

posSRS-TxFH-RRC-Connected-r18 PosSRS-TxFrequencyHoppingRRC-Connected-r18 OPTIONAL,

posSRS-TxFH-RRC-Inactive-r18 PosSRS-TxFrequencyHoppingRRC-Inactive-r18 OPTIONAL,

posSRS-TxFH-WithTimeWindow-r18 ENUMERATED {supported} OPTIONAL,

posSRS-BWA-RRC-Inactive-r18 PosSRS-BWA-RRC-Inactive-r18 OPTIONAL

]]

}

OLPC-SRS-Pos-r16 ::= SEQUENCE {

olpc-SRS-PosBasedOnPRS-Serving-r16 ENUMERATED {supported} OPTIONAL,

olpc-SRS-PosBasedOnSSB-Neigh-r16 ENUMERATED {supported} OPTIONAL,

olpc-SRS-PosBasedOnPRS-Neigh-r16 ENUMERATED {supported} OPTIONAL,

maxNumberPathLossEstimatePerServing-r16 ENUMERATED {n1, n4, n8, n16} OPTIONAL,

...

}

SpatialRelationsSRS-Pos-r16 ::= SEQUENCE {

spatialRelation-SRS-PosBasedOnSSB-Serving-r16 ENUMERATED {supported} OPTIONAL,

spatialRelation-SRS-PosBasedOnCSI-RS-Serving-r16 ENUMERATED {supported} OPTIONAL,

spatialRelation-SRS-PosBasedOnPRS-Serving-r16 ENUMERATED {supported} OPTIONAL,

spatialRelation-SRS-PosBasedOnSRS-r16 ENUMERATED {supported} OPTIONAL,

spatialRelation-SRS-PosBasedOnSSB-Neigh-r16 ENUMERATED {supported} OPTIONAL,

spatialRelation-SRS-PosBasedOnPRS-Neigh-r16 ENUMERATED {supported} OPTIONAL,

...

}

SRS-PosResourcesPerBand-r16 ::= SEQUENCE {

freqBandIndicatorNR-r16 FreqBandIndicatorNR-r16,

maxNumberSRS-PosResourceSetsPerBWP-r16 ENUMERATED {n1, n2, n4, n8, n12, n16},

maxNumberSRS-PosResourcesPerBWP-r16 ENUMERATED {n1, n2, n4, n8, n16, n32, n64},

maxNumberPeriodicSRS-PosResourcesPerBWP-r16 ENUMERATED {n1, n2, n4, n8, n16, n32, n64},

maxNumberAP-SRS-PosResourcesPerBWP-r16 ENUMERATED {n1, n2, n4, n8, n16, n32, n64}

OPTIONAL,

maxNumberSP-SRS-PosResourcesPerBWP-r16 ENUMERATED {n1, n2, n4, n8, n16, n32, n64}

OPTIONAL,

...,

[[

posSRS-BWA-RRC-Connected-r18 PosSRS-BWA-RRC-Connected-r18 OPTIONAL,

posSRS-BWA-IndependentCA-RRC-Connected-r18 PosSRS-BWA-IndependentCA-RRC-Connected-r18

OPTIONAL

]]

}

PosSRS-RRC-Inactive-InInitialUL-BWP-r17 ::= SEQUENCE {

maxNumOfSRSposResourceSets-r17 ENUMERATED {n1, n2, n4, n8, n12, n16 } OPTIONAL,

maxNumOfPeriodicAndSemiPersistentSRSposResources-r17

ENUMERATED {n1, n2, n4, n8, n16, n32, n64 }

OPTIONAL,

maxNumOfPeriodicAndSemiPersistentSRSposResourcesPerSlot-r17

ENUMERATED {n1, n2, n3, n4, n5, n6, n8, n10, n12, n14}

OPTIONAL,

maxNumOfPeriodicSRSposResources-r17

ENUMERATED {n1, n2, n4, n8, n16, n32, n64 }

OPTIONAL,

maxNumOfPeriodicSRSposResourcesPerSlot-r17

ENUMERATED {n1, n2, n3, n4, n5, n6, n8, n10, n12, n14}

OPTIONAL,

dummy1 ENUMERATED {n1, n2, n4, n8, n16, n32, n64} OPTIONAL,

dummy2 ENUMERATED { n1, n2, n3, n4, n5, n6, n8, n10, n12, n14 }

OPTIONAL,

...

}

PosSRS-RRC-Inactive-OutsideInitialUL-BWP-r17 ::= SEQUENCE {

maxSRSposBandwidthForEachSCS-withinCC-FR1-r17

ENUMERATED { mhz5, mhz10, mhz15, mhz20, mhz25, mhz30,  
 mhz35, mhz40, mhz45, mhz50, mhz60, mhz70,

mhz80, mhz90, mhz100 } OPTIONAL,

maxSRSposBandwidthForEachSCS-withinCC-FR2-r17

ENUMERATED {mhz50, mhz100, mhz200, mhz400} OPTIONAL,

maxNumOfSRSposResourceSets-r17 ENUMERATED { n1, n2, n4, n8, n12, n16 } OPTIONAL,

maxNumOfPeriodicSRSposResources-r17 ENUMERATED { n1, n2, n4, n8, n16, n32, n64 }

OPTIONAL,

maxNumOfPeriodicSRSposResourcesPerSlot-r17

ENUMERATED { n1, n2, n3, n4, n5, n6, n8, n10, n12, n14 }

OPTIONAL,

differentNumerologyBetweenSRSposAndInitialBWP-r17

ENUMERATED { supported } OPTIONAL,

srsPosWithoutRestrictionOnBWP-r17

ENUMERATED { supported } OPTIONAL,

maxNumOfPeriodicAndSemiPersistentSRSposResources-r17

ENUMERATED {n1, n2, n4, n8, n16, n32, n64} OPTIONAL,

maxNumOfPeriodicAndSemiPersistentSRSposResourcesPerSlot-r17

ENUMERATED { n1, n2, n3, n4, n5, n6, n8, n10,

n12, n14 } OPTIONAL,

differentCenterFreqBetweenSRSposAndInitialBWP-r17

ENUMERATED { supported } OPTIONAL,

maxNumOfSemiPersistentSRSposResources-r17

ENUMERATED { n1, n2, n4, n8, n16, n32, n64 }

OPTIONAL,

maxNumOfSemiPersistentSRSposResourcesPerSlot-r17

ENUMERATED { n1, n2, n3, n4, n5, n6, n8, n10,

n12, n14 } OPTIONAL,

switchingTimeSRS-TX-OtherTX-r17 ENUMERATED { us100, us140, us200, us300, us500 }

OPTIONAL,

...

}

PosSRS-SP-RRC-Inactive-InInitialUL-BWP-r17 ::= SEQUENCE {

maxNumOfSemiPersistentSRSposResources-r17

ENUMERATED {n1, n2, n4, n8, n16, n32, n64} OPTIONAL,

maxNumOfSemiPersistentSRSposResourcesPerSlot-r17

ENUMERATED {n1, n2, n3, n4, n5, n6, n8, n10, n12, n14}

OPTIONAL,

...

}

PosSRS-TxFrequencyHoppingRRC-Connected-r18 ::= SEQUENCE {

maximumSRS-BandwidthAcrossAllHopsFR1-r18 ENUMERATED {mhz40, mhz50, mhz80, mhz100}

OPTIONAL,

maximumSRS-BandwidthAcrossAllHopsFR2-r18 ENUMERATED {mhz100, mhz200, mhz400} OPTIONAL,

maximumTxFH-Hops-r18 ENUMERATED {n2, n3, n4, n5, n6} OPTIONAL,

rf-TxRetuneTimeFR1-r18 ENUMERATED {n70, n140, n210} OPTIONAL,

rf-TxRetuneTimeFR2-r18 ENUMERATED {n35, n70, n140} OPTIONAL,

switchTimeBetweenActiveBWP-FrequencyHop-r18 ENUMERATED {n100, n140,n200,n300,n500} OPTIONAL,

numOfOverlappingPRB-r18 ENUMERATED {n0, n1, n2, n4} OPTIONAL,

maximumSRS-ResourcePeriodic-r18 ENUMERATED {n1, n2, n4, n8, n16, n32, n64}

OPTIONAL,

maximumSRS-ResourceAperiodic-r18 ENUMERATED {n0, n1, n2, n4, n8, n16, n32, n64}

OPTIONAL,

maximumSRS-ResourceSemipersistent-r18 ENUMERATED {n0, n1, n2, n4, n8, n16, n32, n64}

OPTIONAL,

...

}

PosSRS-TxFrequencyHoppingRRC-Inactive-r18 ::=SEQUENCE {

maximumSRS-BandwidthAcrossAllHopsFR1-r18 ENUMERATED {mhz40, mhz50, mhz80, mhz100}

OPTIONAL,

maximumSRS-BandwidthAcrossAllHopsFR2-r18 ENUMERATED {mhz100, mhz200, mhz400} OPTIONAL,

maximumTxFH-Hops-r18 ENUMERATED {n2, n3, n4, n5, n6} OPTIONAL,

rf-TxRetuneTimeFR1-r18 ENUMERATED {n70, n140, n210} OPTIONAL,

rf-TxRetuneTimeFR2-r18 ENUMERATED {n35, n70, n140} OPTIONAL,

switchTimeBetweenActiveBWP-FrequencyHop-r18 ENUMERATED {n100, n140,n200,n300,n500} OPTIONAL,

numOfOverlappingPRB-r18 ENUMERATED {n0, n1, n2, n4} OPTIONAL,

maximumSRS-ResourcePeriodic-r18 ENUMERATED {n1, n2, n4, n8, n16, n32, n64}

OPTIONAL,

maximumSRS-ResourceSemipersistent-r18 ENUMERATED {n0, n1, n2, n4, n8, n16, n32, n64}

OPTIONAL,

...

}

PosSRS-BWA-RRC-Connected-r18 ::=SEQUENCE {

numOfCarriersIntraBandContiguous-r18 ENUMERATED {two, three, twoandthree},

maximumAggregatedBW-TwoCarriersFR1-r18 ENUMERATED {mhz20, mhz40, mhz50, mhz80, mhz100,

mhz160, mhz180, mhz190, mhz200}

OPTIONAL,

maximumAggregatedBW-TwoCarriersFR2-r18 ENUMERATED {mhz50, mhz100, mhz200, mhz400, mhz600,

mhz800} OPTIONAL,

maximumAggregatedBW-ThreeCarriersFR1-r18 ENUMERATED {mhz80, mhz100, mhz160, mhz200, mhz240,

mhz300} OPTIONAL,

maximumAggregatedBW-ThreeCarriersFR2-r18 ENUMERATED {mhz50, mhz100, mhz200, mhz300, mhz400,

mhz600, mhz800, mhz1000, mhz1200}

OPTIONAL,

maximumAggregatedResourceSet-r18 ENUMERATED {n1, n2, n4, n8, n12, n16},

maximumAggregatedResourcePeriodic-r18 ENUMERATED {n1, n2, n4, n8, n16, n32, n64},

maximumAggregatedResourceAperiodic-r18 ENUMERATED {n0, n1, n2, n4, n8, n16, n32, n64},

maximumAggregatedResourceSemi-r18 ENUMERATED {n0, n1, n2, n4, n8, n16, n32, n64},

maximumAggregatedResourcePeriodicPerSlot-r18

ENUMERATED {n1, n2, n3, n4, n5, n6, n8, n10,

n12, n14},

maximumAggregatedResourceAperiodicPerSlot-r18

ENUMERATED {n0, n1, n2, n3, n4, n5, n6, n8, n10,

n12, n14},

maximumAggregatedResourceSemiPerSlot-r18 ENUMERATED {n0, n1, n2, n3, n4, n5, n6, n8, n10,

n12, n14},

...

}

PosSRS-BWA-IndependentCA-RRC-Connected-r18 ::=SEQUENCE {

numOfCarriersIntraBandContiguous-r18 ENUMERATED {two, three, twoandthree},

maximumAggregatedBW-TwoCarriersFR1-r18 ENUMERATED {mhz20, mhz40, mhz50, mhz80, mhz100,

mhz160, mhz180, mhz190, mhz200}

OPTIONAL,

maximumAggregatedBW-TwoCarriersFR2-r18 ENUMERATED {mhz50, mhz100, mhz200, mhz400, mhz600,

mhz800} OPTIONAL,

maximumAggregatedBW-ThreeCarriersFR1-r18 ENUMERATED {mhz80, mhz100, mhz160, mhz200, mhz240,

mhz300} OPTIONAL,

maximumAggregatedBW-ThreeCarriersFR2-r18 ENUMERATED {mhz50, mhz100, mhz200, mhz300, mhz400,

mhz600, mhz800, mhz1000, mhz1200}

OPTIONAL,

maximumAggregatedResourceSet-r18 ENUMERATED {n1, n2, n4, n8, n12, n16},

maximumAggregatedResourcePeriodic-r18 ENUMERATED {n1, n2, n4, n8, n16, n32, n64},

maximumAggregatedResourceAperiodic-r18 ENUMERATED {n0, n1, n2, n4, n8, n16, n32, n64},

maximumAggregatedResourceSemi-r18 ENUMERATED {n0, n1, n2, n4, n8, n16, n32, n64},

maximumAggregatedResourcePeriodicPerSlot-r18

ENUMERATED {n1, n2, n3, n4, n5, n6, n8, n10,

n12, n14},

maximumAggregatedResourceAperiodicPerSlot-r18

ENUMERATED {n0, n1, n2, n3, n4, n5, n6, n8, n10,

n12, n14},

maximumAggregatedResourceSemiPerSlot-r18 ENUMERATED {n0, n1, n2, n3, n4, n5, n6, n8, n10,

n12, n14},

guardPeriod-r18 ENUMERATED {n0, n30, n100, n140, n200},

powerClassForTwoAggregatedCarriers-r18 ENUMERATED {pc2, pc3} OPTIONAL,

powerClassForThreeAggregatedCarriers-r18 ENUMERATED {pc2, pc3} OPTIONAL,

...

}

PosSRS-BWA-RRC-Inactive-r18 ::=SEQUENCE {

numOfCarriersIntraBandContiguous-r18 ENUMERATED {two, three, twoandthree},

maximumAggregatedBW-TwoCarriersFR1-r18 ENUMERATED {mhz20, mhz40, mhz50, mhz80, mhz100,

mhz160, mhz180, mhz190, mhz200}

OPTIONAL,

maximumAggregatedBW-TwoCarriersFR2-r18 ENUMERATED {mhz50, mhz100, mhz200, mhz400, mhz600,

mhz800} OPTIONAL,

maximumAggregatedBW-ThreeCarriersFR1-r18 ENUMERATED {mhz80, mhz100, mhz160, mhz200, mhz240,

mhz300} OPTIONAL,

maximumAggregatedBW-ThreeCarriersFR2-r18 ENUMERATED {mhz50, mhz100, mhz200, mhz300, mhz400,

mhz600, mhz800, mhz1000, mhz1200}

OPTIONAL,

maximumAggregatedResourceSet-r18 ENUMERATED {n1, n2, n4, n8, n12, n16},

maximumAggregatedResourcePeriodic-r18 ENUMERATED {n1, n2, n4, n8, n16, n32, n64},

maximumAggregatedResourceSemi-r18 ENUMERATED {n0, n1, n2, n4, n8, n16, n32, n64},

maximumAggregatedResourcePeriodicPerSlot-r18

ENUMERATED {n1, n2, n3, n4, n5, n6, n8, n10,

n12, n14},

maximumAggregatedResourceSemiPerSlot-r18 ENUMERATED {n0, n1, n2, n3, n4, n5, n6, n8, n10,

n12, n14},

guardPeriod-r18 ENUMERATED {n0, n30, n100, n140, n200},

powerClassForTwoAggregatedCarriers-r18 ENUMERATED {pc2, pc3} OPTIONAL,

powerClassForThreeAggregatedCarriers-r18 ENUMERATED {pc2, pc3} OPTIONAL,

...

}

-- ASN1STOP

|  |
| --- |
| *NR-UL-SRS-Capability* field descriptions |
| ***srs-PosResourceConfigCA-BandList***  This field indicates the number of SRS for positioning resources supported by the target device. The target device includes this field for each band which belongs to the *srs-CapabilityBandList* for the current configured CA band combination. The capability signalling comprises the following parameters:  - ***freqBandIndicatorNR***indicates the current configured NR band of the target device.  - ***maxNumberSRS-PosResourceSetsPerBWP***indicates the maximum number of SRS Resource Sets for positioning supported by the target device per BWP. Enumerated values *n1*, *n2*, *n4*, *n8*, *n12*, *n16* correspond to 1, 2, 4, 8, 12, 16 SRS Resource Sets for positioning, respectively.  - ***maxNumberSRS-PosResourcesPerBWP***indicates the maximum number of periodic, semi-persistent, and aperiodic SRS Resources for positioning supported by the target device per BWP. Enumerated values *n1, n2, n4, n8, n16, n32, n64* correspond to 1, 2, 4, 8, 16, 32, 64 SRS Resources for positioning, respectively.  - ***maxNumberPeriodicSRS-PosResourcesPerBWP***indicates the maximum number of periodic SRS Resources for positioning supported by the target device per BWP. Enumerated values *n1, n2, n4, n8, n16, n32, n64* correspond to 1, 2, 4, 8, 16, 32, 64 periodic SRS Resources for positioning, respectively.  - ***maxNumberAP-SRS-PosResourcesPerBWP***indicates the maximum number of aperiodic SRS Resources for positioning supported by the target device per BWP. Enumerated values *n1, n2, n4, n8, n16, n32, n64* correspond to 1, 2, 4, 8, 16, 32, 64 aperiodic SRS Resources for positioning, respectively.  - ***maxNumberSP-SRS-PosResourcesPerBWP***indicates the maximum number of semi-persistent SRS Resources for positioning supported by the target device per BWP. Enumerated values *n1, n2, n4, n8, n16, n32, n64* correspond to 1, 2, 4, 8, 16, 32, 64 semi-persistent SRS Resources for positioning, respectively. |
| ***maxNumberSRS-PosPathLossEstimateAllServingCells***  Indicates the maximum number of pathloss estimates that the UE can simultaneously maintain for all the SRS resource sets for positioning across all cells in addition to the up to four pathloss estimates that the UE maintains per serving cell for the PUSCH/PUCCH/SRS transmissions. The UE shall include this field if the UE supports any of *olpc-SRS-PosBasedOnPRS-Serving, olpc-SRS-PosBasedOnSSB-Neigh* and *olpc-SRS-PosBasedOnPRS-Neigh.* Otherwise, the UE does not include this field. |
| ***maxNumberSRS-PosSpatialRelationsAllServingCells***  indicates the maximum number of maintained spatial relations for all the SRS resource sets for positioning across all serving cells in addition to the spatial relations maintained spatial relations per serving cell for the PUSCH/PUCCH/SRS transmissions. It is only applied for FR2. The UE can include this field only if the UE supports any of *spatialRelation-SRS-PosBasedOnSSB-Serving*, *spatialRelation-SRS-PosBasedOnCSI-RS-Serving*, *spatialRelation-SRS-PosBasedOnPRS-Serving*, *spatialRelation-SRS-PosBasedOnSSB-Neigh* or *spatialRelation-SRS-PosBasedOnPRS-Neigh*. Otherwise, the UE does not include this field. |
| ***olpc-SRS-Pos***  Indicates whether the UE supports open-loop power control for SRS for positioning. The capability signalling comprises the following parameters:  - ***olpc-SRS-PosBasedOnPRS-Serving***indicates whether the UE supports OLPC for SRS for positioning based on DL-PRS from the serving cell in the same band. The UE can include this field only if the UE supports NR-DL-*PRS-ProcessingCapability* and *srs-PosResources* TS38.331 [35] Otherwise, the UE does not include this field.  - ***olpc-SRS-PosBasedOnSSB-Neigh***indicates whether the UE supports OLPC for SRS for positioning based on SSB from the neighbouring cell in the same band. The UE can include this field only if the UE supports *srs-PosResources* TS 38.331 [35]. Otherwise, the UE does not include this field.  - ***olpc-SRS-PosBasedOnPRS-Neigh***indicates whether the UE supports OLPC for SRS for positioning based on DL-PRS from the neighbouring cell in the same band. The UE can include this field only if the UE supports *olpc-SRS-PosBasedOnPRS-Serving*. Otherwise, the UE does not include this field.  Note: A DL-PRS from a PRS-only TP is treated as DL-PRS from a non-serving cell.  - ***maxNumberPathLossEstimatePerServing***indicates the maximum number of pathloss estimates that the UE can simultaneously maintain for all the SRS resource sets for positioning per serving cell in addition to the up to four pathloss estimates that the UE maintains per serving cell for the PUSCH/PUCCH/SRS transmissions. The UE shall include this field if the UE supports any of *olpc-SRS-PosBasedOnPRS-Serving, olpc-SRS-PosBasedOnSSB-Neigh* and *olpc-SRS-PosBasedOnPRS-Neigh.* Otherwise, the UE does not include this field. |
| ***spatialRelationsSRS-Pos***  Indicates whether the UE supports spatial relations for SRS for positioning. It is only applicable for FR2. The capability signalling comprises the following parameters:  - ***spatialRelation-SRS-PosBasedOnSSB-Serving*** indicates whether the UE supports spatial relation for SRS for positioning based on SSB from the serving cell in the same band. The UE can include this field only if the UE supports *srs-PosResources* TS 38.331 [35]. Otherwise, the UE does not include this field.  - ***spatialRelation-SRS-PosBasedOnCSI-RS-Serving*** indicates whether the UE supports spatial relation for SRS for positioning based on CSI-RS from the serving cell in the same band. The UE can include this field only if the UE supports *spatialRelation-SRS-PosBasedOnSSB-Serving*. Otherwise, the UE does not include this field.  - ***spatialRelation-SRS-PosBasedOnPRS-Serving***indicates whether the UE supports spatial relation for SRS for positioning based on DL-PRS from the serving cell in the same band. The UE can include this field only if the UE supports any of DL-PRS Resources for DL-AoD, DL-PRS Resources for DL-TDOA or DL-PRS Resources for Multi-RTT, or *srs-PosResources* TS 38.331 [35]. Otherwise, the UE does not include this field.  - ***spatialRelation-SRS-PosBasedOnSRS***indicates whether the UE supports spatial relation for SRS for positioning based on SRS in the same band. The UE can include this field only if the UE supports *srs-PosResources* TS 38.331 [35]. Otherwise, the UE does not include this field.  - ***spatialRelation-SRS-PosBasedOnSSB-Neig****h* indicates whether the UE supports spatial relation for SRS for positioning based on SSB from the neighbouring cell in the same band. The UE can include this field only if the UE supports *spatialRelation-SRS-PosBasedOnSSB-Serving*. Otherwise, the UE does not include this field.  - ***spatialRelation-SRS-PosBasedOnPRS-Neigh***indicates whether the UE supports spatial relation for SRS for positioning based on DL-PRS from the neighbouring cell in the same band. The UE can include this field only if the UE supports *spatialRelation-SRS-PosBasedOnPRS-Serving*. Otherwise, the UE does not include this field.  Note: A DL-PRS from a PRS-only TP is treated as DL-PRS from a non-serving cell. |
| ***posSRS-RRC-Inactive-InInitialUL-BWP***  Indicates whether the UE supports positioning SRS transmission in RRC\_INACTIVE state for initial UL BWP. The capability signalling comprises the following parameters:  - ***maxNumOfSRSposResourceSets*** indicates the maximum number of SRS Resource Sets for positioning supported by the UE.  - ***maxNumOfPeriodicAndSemiPersistentSRSposResources*** indicates the maximum number of periodic and semi-persistent SRS Resources for positioning supported by the UE.  - ***maxNumOfPeriodicAndSemiPersistentSRSposResourcesPerSlot***indicates the maximum number of periodic and semi-persistent SRS Resources for positioning per slot supported by the UE.  - ***maxNumOfPeriodicSRSposResources***indicates the maximum number of periodic SRS Resources for positioning supported by the UE.  - ***maxNumOfPeriodicSRSposResourcesPerSlot***indicates the maximum number of periodic SRS Resources for positioning per slot supported by the UE.  - ***dummy1, dummy2***are not used in the specification. If received they shall be ignored by the receiver. |
| ***posSRS-RRC-Inactive-OutsideInitialUL-BWP***  Indicates whether the UE supports positioning SRS transmission in RRC\_INACTIVE state outside initial UL BWP. The UE can include this field only if the UE supports *posSRS-RRC-Inactive-InInitialUL-BWP*. Otherwise, the UE does not include this field. The capability signalling comprises the following parameters:  - ***maxSRSposBandwidthForEachSCS-withinCC-FR1*** indicates the maximum SRS bandwidth in MHz supported for each SCS that UE supports within a single CC for FR1.  - ***maxSRSposBandwidthForEachSCS-withinCC-FR2*** indicates the maximum SRS bandwidth in MHz supported for each SCS that UE supports within a single CC for FR2.  - ***maxNumOfSRSposResourceSets*** indicates the maximum number of SRS Resource Sets for positioning supported by the UE.  - ***maxNumOfPeriodicSRSposResources***indicates the maximum number of periodic SRS Resources for positioning supported by the UE.  - ***maxNumOfPeriodicSRSposResourcesPerSlot***indicates the maximum number of periodic SRS Resources for positioning per slot supported by the UE.  - ***differentNumerologyBetweenSRSposAndInitialBWP***indicates whether different numerology between the SRS and the initial UL BWP is supported by the UE. If the field is absent, the UE only supports same numerology between the SRS and the initial UL BWP.  - ***srsPosWithoutRestrictionOnBWP*** indicates whether SRS operation without restriction on the BW is supported by the UE; BW of the SRS may not include BW of the CORESET#0 and SSB. If the field is absent, the UE supports only SRS BW that includes the BW of the CORESET #0 and SSB.  - ***maxNumOfPeriodicAndSemiPersistentSRSposResources*** indicates the maximum number of periodic and semi-persistent SRS Resources for positioning supported by the UE.  - ***maxNumOfPeriodicAndSemiPersistentSRSposResourcesPerSlot*** indicates the maximum number of periodic and semi-persistent SRS Resources for positioning per slot supported by the UE.  - ***differentCenterFreqBetweenSRSposAndInitialBWP*** indicates whether different center frequency between the SRS for positioning and the initial UL BWP is supported by the UE. If the field is absent, the UE only supports same center frequency between the SRS for positioning and initial UL BWP.  - ***maxNumOfSemiPersistentSRSposResources***indicates the maximum number of semi-persistent SRS Resources for positioning supported by the UE. The UE can include this field only if the UE supports *posSRS-RRC-Inactive-InInitialUL-BWP*. Otherwise, the UE does not include this field.  - ***maxNumOfSemiPersistentSRSposResourcesPerSlot***indicates the maximum number of semi-persistent SRS Resources for positioning per slot supported by the UE. The UE can include this field only if the UE supports *posSRS-RRC-Inactive-InInitialUL-BWP*. Otherwise, the UE does not include this field.  - ***switchingTimeSRS-TX-OtherTX*** indicates the switching time between SRS Tx and other Tx in initial UL BWP or Rx in initial DL BWP. |
| ***olpc-SRS-PosRRC-Inactive***  Indicates whether the UE supports open-loop power control for SRS for positioning in RRC\_INACTIVE state. The UE can include this field only if the UE supports *posSRS-RRC-Inactive-InInitialUL-BWP*. Otherwise, the UE does not include this field. |
| ***spatialRelationsSRS-PosRRC-Inactive***  Indicates whether the UE supports spatial relations for SRS for positioning in RRC\_INACTIVE state on FR2. The UE can include this field only if the UE supports *posSRS-RRC-Inactive-InInitialUL-BWP*. Otherwise, the UE does not include this field. |
| ***posSRS-SP-RRC-Inactive-InInitialUL-BWP***  Indicates whether the UE supports positioning SRS transmission in RRC\_INACTIVE state for initial UL BWP with semi-persistent SRS. The UE can include this field only if the UE supports *posSRS-RRC-Inactive-InInitialUL-BWP*. Otherwise, the UE does not include this field. The capability signalling comprises the following parameters:  - ***maxNumOfSemiPersistentSRSposResources*** indicates the maximum number of semi-persistent SRS Resources for positioning supported by the UE.  - ***maxNumOfSemiPersistentSRSposResourcesPerSlot*** indicates the maximum number of semi-persistent SRS Resources for positioning per slot supported by the UE. |
| ***posSRS-Preconfigured-RRC-InactiveInitialUL-BWP***  Indicates whether the UE supports pre-configured SRS with validity area in RRC\_INACTIVE for initial UL BWP. The UE can include this field only if the UE supports *posSRS-ValidityAreaRRC-InactiveInitialUL-BWP*. Otherwise, the UE does not include this field. |
| ***posSRS-Preconfigured-RRC-InactiveOutsideInitialUL-BWP***  Indicates whether the UE supports pre-configured SRS with validity area in RRC\_INACTIVE outside initial UL BWP. The UE can include this field only if the UE supports *posSRS-ValidityAreaRRC-InactiveOutsideInitialUL-BWP*. Otherwise, the UE does not include this field. |
| ***posSRS-ValidityAreaRRC-InactiveInitialUL-BWP***  Indicates whether the UE supports SRS for positioning configuration in multi cells in RRC\_INACTIVE for initial UL BWP. The UE can include this field only if the UE support *posSRS-RRC-Inactive-InInitialUL-BWP*. Otherwise, the UE does not include this field. |
| ***posSRS-ValidityAreaRRC-InactiveOutsideInitialUL-BWP***  Indicates whether the UE supports SRS for positioning configuration in multi cells in RRC\_INACTIVE outside initial UL BWP. The UE can include this field only if the UE supports *posSRS-RRC-Inactive-OutsideInitialUL-BWP* and *posSRS-ValidityAreaRRC-InactiveInitialUL-BWP****.*** Otherwise, the UE does not include this field. |
| ***posSRS-TxFH-RRC-Connected***  Indicates the UE capability for support of positioning SRS with Tx frequency hopping in RRC\_CONNECTED for RedCap UEs. The UE can include this field only if the UE supports *SRS-AllPosResources* and one of *supportOfRedCap* and *supportOfERedCap* defined in TS 38.331 [35]. Otherwise, the UE does not include this field. The capability signalling comprises the following parameters:  - ***maximumSRS-BandwidthAcrossAllHopsFR1***: Indicates the maximum positioning SRS bandwidth across all hops in MHz for FR1, which is supported and reported by UE.  - ***maximumSRS-BandwidthAcrossAllHopsFR2***: Indicates the maximum positioning SRS bandwidth across all hops in MHz for FR2, which is supported and reported by UE.  - ***maximumTxFH-Hops***: Indicates the maximum number of transmission hops, which is supported and reported by UE.  - ***rf-TxRetuneTimeFR1***: Indicates the RF Tx retune times between consecutive hops for FR1. Enumerated values indicate 70, 140, 210µs.  - ***rf-TxRetuneTimeFR2***: Indicates the RF Tx retune times between consecutive hops for FR2. Enumerated values indicate 35, 70, 140µs.  - ***switchTimeBetweenActiveBWP-FrequencyHop***: Indicates the switching time between active BWP and frequency hop. Enumerated values indicate 100, 140, 200, 300, 500µs.  - ***numOverlappingPRB***: Indicates the overlapping PRB(s) between adjacent hops. Enumerated values indicate 0,1,2,4 PRBs.  - ***maximumSRS-ResourcePeriodic***: Indicates the maximum number of periodic positioning SRS resources with Tx frequency hopping.  - ***maximumSRS-ResourceAperiodic***: Indicates the maximum number of aperiodic positioning SRS resources with Tx frequency hopping.  - ***maximumSRS-ResourceSemipersistent***: Indicates the maximum number of Semi-persistent positioning SRS resources with Tx frequency hopping.  NOTE 1: No additional UE requirements shall be specified for the case of Tx hopping with non-overlapping hops compared to the case of Tx hopping with overlapping hops, e.g., a UE is not responsible for keeping phase continuity across the hops in either case of overlapping or non-overlapping hops. |
| ***posSRS-TxFH-RRC-Inactive***  Indicates the UE capability for support of positioning SRS with Tx frequency hopping in RRC\_INACTIVE for RedCap UEs. The UE can include this field only if the UE supports *posSRS-RRC-Inactive-OutsideInitialUL-BWP* and one of *supportOfRedCap* and *supportOfERedCap* defined in TS 38.331 [35]. Otherwise, the UE does not include this field. The capability signalling comprises the following parameters:  - ***maximumSRS-BandwidthAcrossAllHopsFR1***: Indicates the maximum positioning SRS bandwidth across all hops in MHz for FR1, which is supported and reported by UE.  - ***maximumSRS-BandwidthAcrossAllHopsFR2***: Indicates the maximum positioning SRS bandwidth across all hops in MHz for FR2, which is supported and reported by UE.  - ***maximumTxFH-Hops***: Indicates the maximum number of transmission hops, which is supported and reported by UE.  - ***rf-TxRetuneTimeFR1***: Indicates the RF Tx retune times between consecutive hops for FR1. Enumerated values indicate 70, 140, 210µs.  - ***rf-TxRetuneTimeFR2***: Indicates the RF Tx retune times between consecutive hops for FR2. Enumerated values indicate 35, 70, 140µs.  - ***switchTimeBetweenActiveBWP-FrequencyHop***: Indicates the switching time between active BWP and frequency hop. Enumerated values indicate 100, 140, 200, 300, 500µs.  - ***numOfOverlappingPRB***: Indicates the overlapping PRB(s) between adjacent hops. Enumerated values indicate 0,1,2,4 PRBs.  - ***maximumSRS-ResourcePeriodic*** indicates the maximum number of periodic positioning SRS resources with Tx frequency hopping.  - ***maximumSRS-ResourceSemipersistent*** indicates the maximum number of Semi-persistent positioning SRS resources with Tx frequency hopping.  NOTE 2: No additional UE requirements shall be specified for the case of Tx hopping with non-overlapping hops compared to the case of Tx hopping with overlapping hops, e.g., a UE is not responsible for keeping phase continuity across the hops in either case of overlapping or non-overlapping hops. |
| ***posSRS-TxFH-WithTimeWindow***  Indicates the UE capability for support of UL time window and transmission of SRS for positioning with Tx Frequency hopping within the window. The UE can include this field only if the UE supports *posSRS-TxFH-RRC-Connected*. Otherwise, the UE does not include this field. |
| ***posSRS-BWA-RRC-Connected***  Indicates the UE capability for support of positioning SRS bandwidth aggregation in RRC\_CONNECTED and comprises the support of the same SRS power reduction across aggregated carriers. The UE can include this field only if the UE supports *SRS-AllPosResources and supportedBandCombinationList* defined in TS 38.331 [35]. Otherwise, the UE does not include this field. The capability signalling comprises the following parameters:  - ***numOfCarriersIntraBandContiguous***: Indicates the number of supported aggregated carriers in intra band contiguous carriers, which is supported and reported by UE.  - ***maximumAggregatedBW-TwoCarriersFR1***: Indicates the maximum aggregated SRS bandwidth in MHz for two aggregated carriers for FR1, which is supported and reported by UE.  - ***maximumAggregatedBW-TwoCarriersFR2***: Indicates the maximum aggregated SRS bandwidth in MHz for two aggregated carriers for FR2, which is supported and reported by UE.  - ***maximumAggregatedBW-ThreeCarriersFR1***: Indicates the maximum aggregated SRS bandwidth in MHz for three aggregated carriers for FR1, which is supported and reported by UE.  - ***maximumAggregatedBW-ThreeCarriersFR2***: Indicates the maximum aggregated SRS bandwidth in MHz for three aggregated carriers for FR2, which is supported and reported by UE.  - ***maximumAggregatedResourceSet***: Indicates the max number of aggregated SRS resource sets for positioning supported by UE for SRS bandwidth aggregation, which is supported and reported by UE.  - ***maximumAggregatedResourcePeriodic***: Indicates the maximum number of aggregated periodic SRS resources for bandwidth aggregation, which is supported and reported by UE.  - ***maximumAggregatedResourceAperiodic***: Indicates the maximum number of aggregated aperiodic SRS resources for bandwidth aggregation, which is supported and reported by UE.  - ***maximumAggregatedResourceSemi***: Indicates the maximum number of aggregated semi-persistent SRS resources for bandwidth aggregation, which is supported and reported by UE.  - ***maximumAggregatedResourcePeriodicPerSlot***: Indicates the maximum number of aggregated periodic SRS resources for bandwidth aggregation per slot, which is supported and reported by UE.  - ***maximumAggregatedResourceAperiodicPerSlot***: Indicates the maximum number of aggregated aperiodic SRS resources for bandwidth aggregation per slot, which is supported and reported by UE.  - ***maximumAggregatedResourceSemiPerSlot***: Indicates the maximum number of aggregated semi-persistent SRS resources for bandwidth aggregation per slot, which is supported and reported by UE.  NOTE 3: The UE supports the simultaneous transmission in a coherent manner of 2 or 3 SRS resources in 2 or 3 intra-band contiguous CCs.  NOTE 4: Each two or three linked SRS resources are counted as 1 resource  NOTE 5: A UE that support *SRS-PosResourceAP* defined in TS 38.331 [35] must signal a non-zero value for *maximumAggregatedResourceAperiodic* and *maximumAggregatedResourceAperiodicPerSlot*;  NOTE 6: UE only reports the number on bands for the current configured CA band combination.  NOTE 6a: For *numOfCarriersIntraBandContiguous*, it shall be less than or equal to the maximum number of the component carrier associated with *ca-BandwidthClassUL-NR* in TS 38.331 [35].  NOTE 6b: For maximum aggregated UL SRS bandwidth, it shall be less than or equal to the maximum aggregated transmission bandwidth associated with *ca-BandwidthClassUL-NR* in TS 38.331 [35]. Additionally, it shall be less than or equal to the maximum aggregated bandwidth for the supported CA configuration in Table 5.5A.1-1 in TS 38.101-1 [37] for FR1 bands or Table 5.5A.1-1 in TS 38.101-2 [34] for FR2 bands for the band where aggregated SRS CCs is configured. |
| ***posSRS-BWA-IndependentCA-RRC-Connected***  Indicates the UE capability for support of positioning SRS bandwidth aggregation independent from UL communication CA in RRC\_CONNECTED and comprises the support of the same SRS power reduction across aggregated carriers. The UE can include this field only if the UE supports *SRS-AllPosResources* defined in TS 38.331 [35]. Otherwise, the UE does not include this field. The capability signalling comprises the following parameters:  - ***numOfCarriersIntraBandContiguous***: Indicates the number of supported aggregated carriers in intra band contiguous carriers, which is supported and reported by UE.  - ***maximumAggregatedBW-TwoCarriersFR1***: Indicates the maximum aggregated SRS bandwidth in MHz for two aggregated carriers for FR1, which is supported and reported by UE.  - ***maximumAggregatedBW-TwoCarriersFR2***: Indicates the maximum aggregated SRS bandwidth in MHz for two aggregated carriers for FR2, which is supported and reported by UE.  - ***maximumAggregatedBW-ThreeCarriersFR1***: Indicates the maximum aggregated SRS bandwidth in MHz for three aggregated carriers for FR1, which is supported and reported by UE.  - ***maximumAggregatedBW-ThreeCarriersFR2***: Indicates the maximum aggregated SRS bandwidth in MHz for three aggregated carriers for FR2, which is supported and reported by UE.  - ***maximumAggregatedResourceSet***: Indicates the max number of aggregated SRS resource sets for positioning supported by UE for SRS bandwidth aggregation, which is supported and reported by UE.  - ***maximumAggregatedResourcePeriodic***: Indicates the maximum number of aggregated periodic SRS resources for bandwidth aggregation, which is supported and reported by UE.  - ***maximumAggregatedResourceAperiodic***: Indicates the maximum number of aggregated aperiodic SRS resources for bandwidth aggregation, which is supported and reported by UE.  - ***maximumAggregatedResourceSemi***: Indicates the maximum number of aggregated semi-persistent SRS resources for bandwidth aggregation, which is supported and reported by UE.  - ***maximumAggregatedResourcePeriodicPerSlot***: Indicates the maximum number of aggregated periodic SRS resources for bandwidth aggregation per slot, which is supported and reported by UE.  - ***maximumAggregatedResourceAperiodicPerSlot***: Indicates the maximum number of aggregated aperiodic SRS resources for bandwidth aggregation per slot, which is supported and reported by UE.  - ***maximumAggregatedResourceSemiPerSlot***: Indicates the maximum number of aggregated semi-persistent SRS resources for bandwidth aggregation per slot, which is supported and reported by UE.  - ***guardPeriod***: Indicates the guard period in microseconds before and after aggregated SRS transmission.  - ***powerClassForTwoAggregatedCarriers***: Indicates the power class of supported two aggregated carriers in intra band contiguous carriers.  - ***powerClassForThreeAggregatedCarriers***: Indicates the power class of supported three aggregated carriers in intra band contiguous carriers.  NOTE 7: The UE supports the simultaneous transmission in a coherent manner of 2 or 3 SRS resources in 2 or 3 intra-band contiguous CCs.  NOTE 8: Each two or three linked SRS resources are counted as 1 resource  NOTE 9: UE only reports the number on bands for the current configured CA band combination.  NOTE 10: Guard period is needed before and after the aggregated SRS transmissions when SRS resource is configured within a CC without PUSCH/PUCCH is linked for aggregation with an SRS resource configured within an UL active BWP of a UL communication CC.  NOTE 11: For a given band, independent of the band combination, the UE must signal the same guard period.  NOTE 12: The power class is only applicable for FR1 bands. |
| ***posSRS-BWA-RRC-Inactive***  Indicates the UE capability for support of positioning SRS bandwidth aggregation in RRC\_INACTIVE and comprises the support of the same SRS power reduction across aggregated carriers. The UE can include this field only if the UE supports *posSRS-RRC-Inactive-OutsideInitialUL-BWP*. Otherwise, the UE does not include this field. If the UE includes this field, the fields *srsPosWithoutRestrictionOnBWP* and *differentCenterFreqBetweenSRSposAndInitialBWP* in *posSRS-RRC-Inactive-OutsideInitialUL-BWP* shall be set to *supported*. The capability signalling comprises the following parameters:  - ***numOfCarriersIntraBandContiguous***: Indicates the number of supported aggregated carriers in intra band contiguous carriers, which is supported and reported by UE.  - ***maximumAggregatedBW-TwoCarriersFR1***: Indicates the maximum aggregated SRS bandwidth in MHz for two aggregated carriers for FR1, which is supported and reported by UE.  - ***maximumAggregatedBW-TwoCarriersFR2***: Indicates the maximum aggregated SRS bandwidth in MHz for two aggregated carriers for FR2, which is supported and reported by UE.  - ***maximumAggregatedBW-ThreeCarriersFR1***: Indicates the maximum aggregated SRS bandwidth in MHz for three aggregated carriers for FR1, which is supported and reported by UE.  - ***maximumAggregatedBW-ThreeCarriersFR2***: Indicates the maximum aggregated SRS bandwidth in MHz for three aggregated carriers for FR2, which is supported and reported by UE.  - ***maximumAggregatedResourceSet***: Indicates the max number of aggregated SRS resource sets for positioning supported by UE for SRS bandwidth aggregation, which is supported and reported by UE.  - ***maximumAggregatedResourcePeriodic***: Indicates the maximum number of aggregated periodic SRS resources for bandwidth aggregation, which is supported and reported by UE.  - ***maximumAggregatedResourceSemi***: Indicates the maximum number of aggregated semi-persistent SRS resources for bandwidth aggregation, which is supported and reported by UE.  - ***maximumAggregatedResourcePeriodicPerSlot***: Indicates the maximum number of aggregated periodic SRS resources for bandwidth aggregation per slot, which is supported and reported by UE.  - ***maximumAggregatedResourceSemiPerSlot***: Indicates the maximum number of aggregated semi-persistent SRS resources for bandwidth aggregation per slot, which is supported and reported by UE.  - ***guardPeriod***: Indicates the guard period in microseconds before and after aggregated SRS transmission.  - ***powerClassForTwoAggregatedCarriers***: Indicates the power class of supported two aggregated carriers in intra band contiguous carriers.  - ***powerClassForThreeAggregatedCarriers***: Indicates the power class of supported three aggregated carriers in intra band contiguous carriers.  NOTE 13: The power class is only applicable for FR1 bands. |

#### *– NR-PhaseQuality*

The IE *NR-PhaseQuality* defines the quality of the RSCP/RSCPD measurement.

-- ASN1START

NR-PhaseQuality-r18 ::= SEQUENCE {

phaseQualityIndex-r18 INTEGER (0..179),

phaseQualityResolution-r18 ENUMERATED {mdot1, m1,...},

...

}

-- ASN1STOP

| *NR-PhaseQuality* field descriptions |
| --- |
| ***phaseQualityIndex***  This field provides an index value for an estimate of the uncertainty of the reported phase for which the IE *NR-PhaseQuality* is provided in units of degrees. |
| ***phaseQualityResolution***  This field provides the resolution used in the *phaseQualityIndex* field. Enumerated values *mdot1* and *m1* correspond to 0.1 and 1 degrees respectively. |

#### – *ReferencePoint*

The IE *ReferencePoint* provides a well-defined location relative to which other locations may be defined.

-- ASN1START

ReferencePoint-r16 ::= SEQUENCE {

referencePointGeographicLocation-r16 CHOICE {

location3D-r16 EllipsoidPointWithAltitudeAndUncertaintyEllipsoid,

ha-location3D-r16 HighAccuracyEllipsoidPointWithAltitudeAndUncertaintyEllipsoid-r15,

...,

localOrigin-v1800 LocalOrigin-r18

},

...

}

-- ASN1STOP

| *ReferencePoint* field descriptions |
| --- |
| ***referencePointGeographicLocation***  This field provides the geodetic or local location of the reference point. |
| ***localOrigin***  This field provides an identifier for the reference point that defines the origin and orientation of a local Cartesian coordinate system [15]. |

#### – *RelativeCartesianLocation*

The IE *RelativeCartesianLocation* provides a Cartesian location relative to some known reference location in a local coordinate system defined by a local origin.

-- ASN1START

RelativeCartesianLocation-r18 ::= SEQUENCE {

cartesianCoordinatesUnits-r18 ENUMERATED { mm, cm, dm, m, ...},

x-value-r18 X-Value-r18,

y-value-r18 Y-Value-r18,

z-value-r18 Z-Value-r18,

locationUnc-r18 LocationUncertainty-r16 OPTIONAL, -- Need OP

...

}

X-Value-r18 ::= SEQUENCE {

delta-x-r18 INTEGER (-1024..1023),

coarse-delta-x-r18 INTEGER (0..4095) OPTIONAL, -- Need OP

...

}

Y-Value-r18 ::= SEQUENCE {

delta-y-r18 INTEGER (-1024..1023),

coarse-delta-y-r18 INTEGER (0..4095) OPTIONAL, -- Need OP

...

}

Z-Value-r18 ::= SEQUENCE {

delta-z-r18 INTEGER (-1024..1023),

coarse-delta-z-r18 INTEGER (0..4095) OPTIONAL, -- Need OP

...

}

-- ASN1STOP

|  |
| --- |
| *RelativeCartesianLocation* field descriptions |
| ***cartesianCoordinatesUnits***  This field provides the units and scale factor for the *x-value,* *y-value* and *z-value* fields. Enumerated values *mm*, *cm*, *dm*, and *m*, correspond to 10-3 metre, 10-2 metre, 10-1 metre and 1 metres, respectively. |
| ***x-value***  This field specifies the x-value of the desired location in a Cartesian coordinate system defined by an associated *LocalOrigin* IE and comprises the following sub-fields:  - ***delta-x*** specifies the delta value on the x-axis of a Cartesian coordinate system in the unit provided in *cartesianCoordinatesUnits* field.  - ***coarse-delta-x*** specifies the delta value on the x-axis of a Cartesian coordinate system in 1024 times the size of the unit provided in *cartesianCoordinatesUnits* field and with the same sign as in the *delta-x* field. If this field is absent, the value for *coarse-delta-x*is zero.  I.e., the full *x-value* is given by:  (*delta-x* × *cartesianCoordinatesUnits*)±(*coarse-delta-x* × 1024 × *cartesianCoordinatesUnits*) [m].  Positive value represents easting from reference point (local origin), unless the field *horizAxesOrientation* is provided in the associated *LocalOrigin* IE, in which case the local coordinate system is rotated clockwise horizontally by *horizAxesOrientation*). |
| ***y-value***  This field specifies the y-value of the desired location in a Cartesian coordinate system defined by an associated *LocalOrigin* IE and comprises the following sub-fields:  - ***delta-y*** specifies the delta value on the y-axis of a Cartesian coordinate system in the unit provided in *cartesianCoordinatesUnits* field.  - ***coarse-delta-y*** specifies the delta value on the y-axis of a Cartesian coordinate system in 1024 times the size of the unit provided in *cartesianCoordinatesUnits* field and with the same sign as in the *delta-y* field. If this field is absent, the value for *coarse-delta-y*is zero.  I.e., the full *y-value* is given by:  (*delta-y* × *cartesianCoordinatesUnits*)±(*coarse-delta-y* × 1024 × *cartesianCoordinatesUnits*) [m].  Positive value represents northing from reference point (local origin), unless the field *horizAxesOrientation* is provided in the associated *LocalOrigin* IE, in which case the local coordinate system is rotated clockwise horizontally by *horizAxesOrientation*). |
| ***z-value***  This field specifies the z-value of the desired location in a Cartesian coordinate system and comprises the following sub-fields:  - ***delta-z*** specifies the delta value on the z-axis of a Cartesian coordinate system in the unit provided in *cartesianCoordinatesUnits* field.  - ***coarse-delta-z*** specifies the delta value on the z-axis of a Cartesian coordinate system in 1024 times the size of the unit provided in *cartesianCoordinatesUnits* field and with the same sign as in the *delta-z* field. If this field is absent, the value for *coarse-delta-z*is zero.  I.e., the full *z-value* is given by:  (*delta-z* × *cartesianCoordinatesUnits*)±(*coarse-delta-z* × 1024 × *cartesianCoordinatesUnits*) [m]. |
| ***locationUnc***  This field specifies the uncertainty of the location coordinates (see IE *RelativeLocation*).  If this field is absent, the uncertainty is the same as for the associated reference point location. |

#### – *RelativeLocation*

The IE *RelativeLocation* provides a location relative to some known reference location.

-- ASN1START

RelativeLocation-r16 ::= SEQUENCE {

milli-arc-second-units-r16 ENUMERATED { mas0-03, mas0-3, mas3, mas30, ...},

height-units-r16 ENUMERATED {mm, cm, m, ...},

delta-latitude-r16 Delta-Latitude-r16,

delta-longitude-r16 Delta-Longitude-r16,

delta-height-r16 Delta-Height-r16,

locationUNC-r16 LocationUncertainty-r16 OPTIONAL, -- Need OP

...

}

Delta-Latitude-r16 ::= SEQUENCE {

delta-Latitude-r16 INTEGER (-1024..1023),

coarse-delta-Latitude-r16 INTEGER (0..4095) OPTIONAL, -- Need OP

...

}

Delta-Longitude-r16 ::= SEQUENCE {

delta-Longitude-r16 INTEGER (-1024..1023),

coarse-delta-Longitude-r16 INTEGER (0..4095) OPTIONAL, -- Need OP

...

}

Delta-Height-r16 ::= SEQUENCE {

delta-Height-r16 INTEGER (-1024..1023),

coarse-delta-Height-r16 INTEGER (0..4095) OPTIONAL, -- Need OP

...

}

LocationUncertainty-r16 ::= SEQUENCE {

horizontalUncertainty-r16 INTEGER (0..255),

horizontalConfidence-r16 INTEGER (0..100),

verticalUncertainty-r16 INTEGER (0..255),

verticalConfidence-r16 INTEGER (0..100)

}

-- ASN1STOP

|  |
| --- |
| *RelativeLocation* field descriptions |
| ***milli-arc-second-units***  This field provides the units and scale factor for the *delta-latitude* and *delta-longitude* fields. Enumerated values *mas0-03*, *mas0-3*, *mas3*, and *mas30*, correspond to 0.03, 0.3, 3, and 30 milliarcseconds, respectively. |
| ***height-units***  This field provides the units and scale factor for the *delta-height* field. Enumerated values *mm*, *cm*, and *m* correspond to 10-3 metre, 10-2 metre, and 1 metres, respectively. |
| ***delta-latitude***  This field specifies the delta value in latitude of the desired location, defined as "desired location" minus "reference point location" and comprises the following sub-fields:  - ***delta-Latitude*** specifies the delta value in latitude in the unit provided in *milli-arc-second-units* field.  - ***coarse-delta-Latitude*** specifies the delta value in latitude in 1024 times the size of the unit provided in *milli-arc‑second‑units* field and with the same sign as in the *delta-Latitude* field. If this field is absent, the value for *coarse-delta-Latitude*is zero.  I.e., the full *delta-latitude* is given by:  (*delta-Latitude* × *milli-arc-second-units*)±(*coarse-delta-Latitude* × 1024 × *milli-arc-second-units*) [milli-arc-seconds] |
| ***delta-longitude***  This field specifies the delta value in longitude of the desired location, defined as "desired location" minus "reference point location" and comprises the following sub-fields:  - ***delta-Longitude*** specifies the delta value in longitude in the unit provided in *milli-arc-second-units* field.  - ***coarse-delta-Longitude*** specifies the delta value in longitude in 1024 times the size of the unit provided in *milli-arc‑second‑units* field and with the same sign as in the *delta-Longitude* field. If this field is absent, the value for *coarse-delta-Longitude*is zero.  I.e., the full *delta-longitude* is given by:  (*delta-Longitude* × *milli-arc-second-units*)±(*coarse-delta-Latitude* × 1024 × *milli-arc-second-units*) [milli-arc-seconds] |
| ***delta-height***  This field specifies the delta value in ellipsoidal height of the desired location, defined as "desired location" minus "reference point location" and comprises the following sub-fields:  - ***delta-Height*** specifies the delta value in ellipsoidal height in the unit provided in *height-units* field.  - ***coarse-delta-Height*** specifies the delta value in ellipsoidal height in 1024 times the size of the unit provided in *height-units* field and with the same sign as in the *delta-Height* field. If this field is absent, the value for *coarse-delta-Height*is zero.  I.e., the full *delta-height* is given by:  (*delta-Height* × *height-units*) *±* (*coarse-delta-Height* × 1024 × *height-units*) [metres] |
| ***locationUNC***  This field specifies the uncertainty of the location coordinates and comprises the following sub-fields:  - ***horizontalUncertainty*** indicates the horizontal uncertainty of the ARP latitude/longitude. The ′*horizontalUncertainty*′ corresponds to the encoded high accuracy uncertainty as defined in TS 23.032 [15] and ′*horizontalConfidence*′ corresponds to confidence as defined in TS 23.032 [15].  - ***verticalUncertainty*** indicates the vertical uncertainty of the ARP altitude. The '*verticalUncertainty*' corresponds to the encoded high accuracy uncertainty as defined in TS 23.032 [15] and '*verticalConfidence*' corresponds to confidence as defined in TS 23.032 [15].  If this field is absent, the uncertainty is the same as for the associated reference point location. |

#### – *TEG-TimingErrorMargin*

The IE *TEG-TimingErrorMargin* defines the timing error margin values of the UE Rx TEGs, UE Tx TEGs, or TRP Tx TEGs. Enumerated value '*tc0*' corresponds to 0 Tc, '*tc2*' corresponds to 2 Tc and so on, where Tc is defined in TS 38.211 [41] clause 4.1.

-- ASN1START

TEG-TimingErrorMargin-r17 ::= ENUMERATED { tc0, tc2, tc4, tc6, tc8, tc12, tc16, tc20, tc24,

tc32, tc40, tc48, tc56, tc64, tc72, tc80 }

-- ASN1STOP

#### – *RxTxTEG-TimingErrorMargin*

The IE *RxTxTEG-TimingErrorMargin* defines the timing error margin values of the UE RxTx TEGs. Enumerated value '*tc0-5*' corresponds to 0.5 Tc, '*tc1*' corresponds to 1 Tc and so on, where Tc is defined in TS 38.211 [41] clause 4.1.

-- ASN1START

RxTxTEG-TimingErrorMargin-r17 ::= ENUMERATED { tc0-5, tc1, tc2, tc4, tc8, tc12, tc16, tc20,

tc24, tc32, tc40, tc48, tc64, tc80, tc96, tc128 }

-- ASN1STOP

## 6.5 Positioning Method IEs

### 6.5.1 OTDOA Positioning

This clause defines the information elements for downlink OTDOA positioning, which includes TBS positioning based on PRS signals (TS 36.305 [2]).

#### 6.5.1.1 OTDOA Assistance Data

#### – *OTDOA-ProvideAssistanceData*

The IE *OTDOA-ProvideAssistanceData* is used by the location server to provide assistance data to enable UE‑assisted downlink OTDOA. It may also be used to provide OTDOA positioning specific error reason.

Throughout clause 6.5.1, "assistance data reference cell" refers to the cell defined by the IE *OTDOA-ReferenceCellInfo* and"NB-IoT assistance data reference cell" refers to the cell defined by the IE *OTDOA-ReferenceCellInfoNB* (see clause 6.5.1.2). "RSTD reference cell" applies only in clause 6.5.1.5.

If both IEs, *OTDOA-ReferenceCellInfo* and *OTDOA-ReferenceCellInfoNB* are included in *OTDOA‑ProvideAssistanceData*, the assistance data reference cell and NB-IoT assistance data reference cell correspond to the same cell, and the target device may assume that PRS and NPRS antenna ports are quasi co-located, as defined in TS 36.211 [16].

Throughout clause 6.5.1, the term "cell" refers to "transmission point (TP)", unless distinguished in the field description.

NOTE 1: The location server should include at least one cell for which the SFN can be obtained by the target device, e.g. the serving cell, in the assistance data, either as the assistance data reference cell or in the neighbour cell list. Otherwise the target device will be unable to perform the OTDOA measurement and the positioning operation will fail.

NOTE 2: Due to support of cells containing multiple TPs and PRS-only TPs not associated with cells, the term "cell" as used in clause 6.5.1 may not always correspond to a cell for the E-UTRAN.

NOTE 3: For NB-IoT access, due to support of NPRS on multiple carriers, the term "cell" as used in clause 6.5.1 refers to the anchor carrier, unless otherwise stated.

-- ASN1START

OTDOA-ProvideAssistanceData ::= SEQUENCE {

otdoa-ReferenceCellInfo OTDOA-ReferenceCellInfo OPTIONAL, -- Need ON

otdoa-NeighbourCellInfo OTDOA-NeighbourCellInfoList OPTIONAL, -- Need ON

otdoa-Error OTDOA-Error OPTIONAL, -- Need ON

...,

[[

otdoa-ReferenceCellInfoNB-r14 OTDOA-ReferenceCellInfoNB-r14 OPTIONAL, -- Need ON

otdoa-NeighbourCellInfoNB-r14 OTDOA-NeighbourCellInfoListNB-r14 OPTIONAL -- Need ON

]]

}

-- ASN1STOP

#### 6.5.1.2 OTDOA Assistance Data Elements

#### – *OTDOA-ReferenceCellInfo*

The IE *OTDOA-ReferenceCellInfo* is used by the location server to provide assistance data reference cell information for OTDOA assistance data. The slot number offsets and expected RSTDs in *OTDOA-NeighbourCellInfoList* are provided relative to the cell defined by this IE. If *earfcnRef* of this assistance data reference cell is different from that of the serving cell, the LPP layer shall inform lower layers to start performing inter-frequency RSTD measurements with this cell and provide to lower layers the information about this assistance data reference cell, e.g. EARFCN and PRS positioning occasion information.

NOTE: The location server should always include the PRS configuration of the assistance data reference and neighbour cells. Otherwise the UE may not meet the accuracy requirements as defined in TS 36.133 [18].

-- ASN1START

OTDOA-ReferenceCellInfo ::= SEQUENCE {

physCellId INTEGER (0..503),

cellGlobalId ECGI OPTIONAL, -- Need ON

earfcnRef ARFCN-ValueEUTRA OPTIONAL, -- Cond NotSameAsServ0

antennaPortConfig ENUMERATED {ports1-or-2, ports4, ... }

OPTIONAL, -- Cond NotSameAsServ1

cpLength ENUMERATED { normal, extended, ... },

prsInfo PRS-Info OPTIONAL, -- Cond PRS

...,

[[ earfcnRef-v9a0 ARFCN-ValueEUTRA-v9a0 OPTIONAL -- Cond NotSameAsServ2

]],

[[ tpId-r14 INTEGER (0..4095) OPTIONAL, -- Need ON

cpLengthCRS-r14 ENUMERATED { normal, extended, ... }

OPTIONAL, -- Cond CRS

sameMBSFNconfigRef-r14 BOOLEAN OPTIONAL, -- Need ON

dlBandwidth-r14 ENUMERATED {n6, n15, n25, n50, n75, n100}

OPTIONAL, -- Cond NotSameAsServ3

addPRSconfigRef-r14 SEQUENCE (SIZE (1..maxAddPRSconfig-r14)) OF PRS-Info

OPTIONAL -- Need ON

]],

[[

nr-LTE-SFN-Offset-r15 INTEGER (0..1023) OPTIONAL -- Cond NR

]],

[[

tdd-config-v1520 TDD-Config-v1520 OPTIONAL, -- Need ON

nr-LTE-fineTiming-Offset-r15 INTEGER (0..19) OPTIONAL -- Cond FineOffset

]]

}

maxAddPRSconfig-r14 INTEGER ::= 2

-- ASN1STOP

| Conditional presence | Explanation |
| --- | --- |
| *NotSameAsServ0* | This field is absent if *earfcnRef-v9a0* is present. Otherwise, the field is mandatory present if the EARFCN of the OTDOA assistance data reference cell is not the same as the EARFCN of the target devices' current primary cell. |
| *NotSameAsServ1* | The field is mandatory present if the antenna port configuration of the OTDOA assistance data reference cell is not the same as the antenna port configuration of the target devices' current primary cell. |
| *NotSameAsServ2* | The field is absent if *earfcnRef* is present. Otherwise, the field is mandatory present if the EARFCN of the OTDOA assistance data reference cell is not the same as the EARFCN of the target devices' current primary cell. |
| *PRS* | The field is mandatory present if positioning reference signals are available in the assistance data reference cell (TS 36.211 [16]); otherwise it is not present. |
| *CRS* | The field is optionally present, need ON, if *prsInfo* is present. Otherwise it is not present. |
| *NotSameAsServ3* | The field is mandatory present if the downlink bandwidth configuration of the assistance data reference cell is not the same as the downlink bandwidth configuration of the target devices' current primary cell and if PRS frequency hopping is used in the assistance data reference cell (TS 36.211 [16]); otherwise it is not present. |
| *NR* | The field is optionally present, need ON, if the target device is served by an NR cell; otherwise it is not present. |
| *FineOffset* | The field is optionally present, need ON, if *nr-LTE-SFN-Offset* is present. Otherwise it is not present. |

| *OTDOA-ReferenceCellInfo* field descriptions |
| --- |
| ***physCellId***  This field specifies the physical cell identity of the assistance data reference cell, as defined in TS 36.331 [12]. |
| ***cellGlobalId***  This field specifies the ECGI, the globally unique identity of a cell in E-UTRA, of the assistance data reference cell, as defined in TS 36.331 [12]. The server should include this field if it considers that it is needed to resolve ambiguity in the cell indicated by *physCellId*. |
| ***earfcnRef***  This field specifies the EARFCN of the assistance data reference cell. |
| ***antennaPortConfig***  This field specifies whether 1 (or 2) antenna port(s) or 4 antenna ports for cell specific reference signals (CRS) are used in the assistance data reference cell. |
| ***cpLength***  This field specifies the cyclic prefix length of the assistance data reference cell PRS if the *prsInfo* field is present, otherwise this field specifies the cyclic prefix length of the assistance data reference cell CRS. |
| ***prsInfo***  This field specifies the first PRS configuration of the assistance data reference cell. |
| ***tpId***  This field specifies an identity of the transmission point. This field together with the *physCellId* and/or *prsID* may be used to identify the transmission point in the case the same physical cell ID is shared by multiple transmission points. |
| ***cpLengthCRS***  This field specifies the cyclic prefix length of the assistance data reference cell CRS. If this field is present, the target device may assume the CRS and PRS antenna ports of the assistance data reference cell are quasi co-located (as defined in TS 36.211 [16]). |
| ***sameMBSFNconfigRef***  This field indicates whether the MBSFN subframe configuration of the assistance data reference cell is the same as the current primary cell of the target device. TRUE means the same, and FALSE means not the same. |
| ***dlBandwidth***  This field specifies the downlink bandwidth configuration of the assistance data reference cell, NRB in downlink, see TS 36.101 [21, table 5.6-1]. Enumerated value n6 corresponds to 6 resource blocks, n15 to 15 resource blocks and so on. |
| ***addPRSconfigRef***  This field specifies the additional (second and possibly third) PRS configuration(s) of the assistance data reference cell. |
| ***nr-LTE-SFN-Offset***  This field specifies the SFN offset between the serving NR cell and the LTE assistance data reference cell.  The offset corresponds to the number of full radio frames counted from the beginning of a radio frame #0 of the NR serving cell to the beginning of the closest subsequent radio frame #0 of the assistance data reference cell. |
| ***tdd-config***  This field specifies the TDD specific physical channel configuration of the assistance data reference cell. The field should be present if the assistance data reference cell is a TDD cell and if the TDD UL/DL configuration of the assistance data reference cell is not the same as the target devices' current primary cell or if the target devices' current primary cell is a FDD cell. |
| ***nr-LTE-fineTiming-Offset***  This field specifies the frame boundary offset between the NR serving cell and the LTE assistance data reference cell in units of 0.5 ms. The offset is counted from the beginning of a subframe #0 of the NR serving cell to the beginning of the closest subsequent subframe #0 of the LTE assistance data reference cell, rounded down to multiples of 0.5 ms. Value 0 corresponds to 0 ms, value 1 corresponds to 0.5 ms, 2 to 1 ms and so on. |

#### – *PRS-Info*

The IE *PRS-Info* provides the information related to the configuration of PRS in a cell.

-- ASN1START

PRS-Info ::= SEQUENCE {

prs-Bandwidth ENUMERATED { n6, n15, n25, n50, n75, n100, ... },

prs-ConfigurationIndex INTEGER (0..4095),

numDL-Frames ENUMERATED {sf-1, sf-2, sf-4, sf-6, ..., sf-add-v1420},

...,

prs-MutingInfo-r9 CHOICE {

po2-r9 BIT STRING (SIZE(2)),

po4-r9 BIT STRING (SIZE(4)),

po8-r9 BIT STRING (SIZE(8)),

po16-r9 BIT STRING (SIZE(16)),

...,

po32-v1420 BIT STRING (SIZE(32)),

po64-v1420 BIT STRING (SIZE(64)),

po128-v1420 BIT STRING (SIZE(128)),

po256-v1420 BIT STRING (SIZE(256)),

po512-v1420 BIT STRING (SIZE(512)),

po1024-v1420 BIT STRING (SIZE(1024))

} OPTIONAL, -- Need OP

[[ prsID-r14 INTEGER (0..4095) OPTIONAL, -- Need ON

add-numDL-Frames-r14 INTEGER (1..160) OPTIONAL, -- Cond sf-add

prsOccGroupLen-r14 ENUMERATED {g2, g4, g8, g16, g32, g64, g128,... }

OPTIONAL, -- Cond Occ-Grp

prsHoppingInfo-r14 CHOICE {

nb2-r14 INTEGER (0.. maxAvailNarrowBands-Minus1-r14),

nb4-r14 SEQUENCE (SIZE (3))

OF INTEGER (0.. maxAvailNarrowBands-Minus1-r14)

} OPTIONAL -- Cond PRS-FH

]]

}

maxAvailNarrowBands-Minus1-r14 INTEGER ::= 15 -- Maximum number of narrowbands minus 1

-- ASN1STOP

| Conditional presence | Explanation |
| --- | --- |
| *sf-add* | The field is mandatory present if the *numDL-Frames* field has the value '*sf-add*'; otherwise it is not present. |
| *Occ-Grp* | The field is mandatory present if a PRS occasion group is configured; otherwise it is not present. |
| *PRS-FH* | The field is mandatory present if frequency hopping is used for PRS; otherwise it is not present. |

| *PRS-Info* field descriptions |
| --- |
| ***prs-Bandwidth***  This field specifies the bandwidth that is used to configure the positioning reference signals on. Enumerated values are specified in number of resource blocks (n6 corresponds to 6 resource blocks, n15 to 15 resource blocks and so on) and define 1.4, 3, 5, 10, 15 and 20 MHz bandwidth. |
| ***prs-ConfigurationIndex***  This field specfies the positioning reference signals configuration index IPRS as defined in TS 36.211 [16]. |
| ***numDL-Frames***  This field specifies the number of consecutive downlink subframes NPRS with positioning reference signals, as defined in TS 36.211 [16]. Enumerated values define 1, 2, 4, or 6 consecutive downlink subframes. The value *sf-add* indicates that NPRS is provided in the field *add-numDL-Frames.* |
| ***prs-MutingInfo***  This field specifies the PRS muting configuration of the cell. The PRS muting configuration is defined by a periodic PRS muting sequence with periodicity TREP where TREP, counted in the number of PRS occasion groups (TS 36.133 [18]), can be 2, 4, 8, 16, 32, 64, 128, 256, 512, or 1024 which is also the length of the selected bit string that represents this PRS muting sequence. If a bit in the PRS muting sequence is set to "0", then the PRS is muted in all the PRS occasions in the corresponding PRS occasion group. A PRS occasion group comprises one or more PRS occasions as indicated by *prsOccGroupLen*. Each PRS occasion comprises NPRS downlink positioning subframes as defined in TS 36.211 [16]. The first bit of the PRS muting sequence corresponds to the first PRS occasion group that starts after the beginning of the assistance data reference cell SFN=0. The sequence is valid for all subframes after the target device has received the *prs-MutingInfo*. If this field is not present the target device may assume that the PRS muting is not in use for the cell.  When the SFN of the assistance data reference cell is not known to the UE and *prs-MutingInfo* is provided for a cell in the *OTDOA-NeighbourCellInfoList* IE, the UE may assume no PRS is transmitted by that cell.  When the UE receives a TREP-bit muting pattern together with a PRS periodicity TPRS for the same cell which exceeds 10240 subframes (i.e., TREP × TPRS > 10240 subframes), the UE shall assume an n-bit muting pattern based on the first n‑bits, where n = 10240/TPRS. |
| ***prsID***  This field specifies the PRS-ID as defined in TS 36.211 [16]. |
| ***add-numDL-Frames***  This field specifies the number of consecutive downlink subframes NPRS with positioning reference signals, as defined in TS 36.211 [16]. Integer values define 1, 2, 3, …, 160 consecutive downlink subframes. |
| ***prsOccGroupLen***  This field specifies the PRS occasion group length, defined as the number of consecutive PRS occasions comprising a PRS occasion group. Each PRS occasion of the PRS occasion group consists of *numDL-Frames* or *add-numDL-Frames* consecutive downlink subframes with positioning reference signals. Enumerated values define 2, 4, 8, 16, 32, 64 or 128 consecutive PRS occasions. If omitted, the PRS occasion group length is 1. The product of the PRS periodicity T\_PRS from the prs-ConfigurationIndex and the PRS occasion group length cannot exceed 1280. |
| ***prsHoppingInfo***  This field specifies the PRS frequency hopping configuration (TS 36.211 [16]). The choice nb2 indicates hopping between 2 narrowbands; the choice nb4 indicates hopping between 4 narrowbands. The first PRS positioning occasion of the first PRS occasion group that starts after the beginning of SFN=0 of the assistance data reference cell is located at the centre of the system bandwidth. The frequency band of each subsequent PRS occasion is indicated by nb2 or nb4, respectively, which defines the narrowband index as specified in TS 36.211 [16]. If this field is absent, no PRS frequency hopping is used. |

#### – *TDD-Config*

The IE *TDD-Config* is used to specify the TDD specific physical channel configuration.

-- ASN1START

TDD-Config-v1520 ::= SEQUENCE {

subframeAssignment-v1520 ENUMERATED { sa0, sa1, sa2, sa3, sa4, sa5, sa6 },

...

}

-- ASN1STOP

| *TDD-Config* field descriptions |
| --- |
| ***subframeAssignment***  This field specifies the TDD UL/DL subframe configuration where *sa0* points to Configuration 0, *sa1* to Configuration 1 etc. as specified in TS 36.211 [16], table 4.2-2. The target device assumes the same value for all assistance data cells residing on same frequency band. |

#### – *OTDOA-NeighbourCellInfoList*

The IE *OTDOA-NeighbourCellInfoList* is used by the location server to provide neighbour cell information for OTDOA assistance data. If the target device is not capable of supporting additional neighbour cells (as indicated by the absence of the IE *additionalNeighbourCellInfoList* in *OTDOA-ProvideCapabilities*), the set of cells in the *OTDOA-NeighbourCellInfoList* is grouped per frequency layer and in the decreasing order of priority for measurement to be performed by the target device, with the first cell in the list being the highest priority for measurement and with the same *earfcn* not appearing in more than one instance of *OTDOA‑NeighbourFreqInfo*.

If the target device is capable of supporting additional neighbour cells (as indicated by the presence of the IE *additionalNeighbourCellInfoList* in *OTDOA-ProvideCapabilities*)*,* the list may contain all cells (up to 3x24 cells) belonging to the same frequency layer or cells from different frequency layers with the first cell in the list still being the highest priority for measurement.

The prioritization of the cells in the list is left to server implementation. The target device should provide the available measurements in the same order as provided by the server.

If inter-frequency neighbour cells are included in *OTDOA-NeighbourCellInfoList*, where an inter-frequency is a E-UTRA frequency which is different from the E-UTRA serving cell frequency, the LPP layer shall inform lower layers to start performing inter-frequency RSTD measurements for these neighbour cells and also provide to lower layers the information about these neighbour cells, e.g. EARFCN and PRS positioning occasion information.

-- ASN1START

OTDOA-NeighbourCellInfoList ::= SEQUENCE (SIZE (1..maxFreqLayers)) OF OTDOA-NeighbourFreqInfo

OTDOA-NeighbourFreqInfo ::= SEQUENCE (SIZE (1..24)) OF OTDOA-NeighbourCellInfoElement

OTDOA-NeighbourCellInfoElement ::= SEQUENCE {

physCellId INTEGER (0..503),

cellGlobalId ECGI OPTIONAL, -- Need ON

earfcn ARFCN-ValueEUTRA OPTIONAL, -- Cond NotSameAsRef0

cpLength ENUMERATED {normal, extended, ...}

OPTIONAL, -- Cond NotSameAsRef1

prsInfo PRS-Info OPTIONAL, -- Cond NotSameAsRef2

antennaPortConfig ENUMERATED {ports-1-or-2, ports-4, ...}

OPTIONAL, -- Cond NotsameAsRef3

slotNumberOffset INTEGER (0..19) OPTIONAL, -- Cond NotSameAsRef4

prs-SubframeOffset INTEGER (0..1279) OPTIONAL, -- Cond InterFreq

expectedRSTD INTEGER (0..16383),

expectedRSTD-Uncertainty INTEGER (0..1023),

...,

[[ earfcn-v9a0 ARFCN-ValueEUTRA-v9a0 OPTIONAL -- Cond NotSameAsRef5

]],

[[ tpId-r14 INTEGER (0..4095) OPTIONAL, -- Need ON

prs-only-tp-r14 ENUMERATED { true } OPTIONAL, -- Cond TBS

cpLengthCRS-r14 ENUMERATED { normal, extended, ... }

OPTIONAL, -- Cond CRS

sameMBSFNconfigNeighbour-r14 BOOLEAN OPTIONAL, -- Need ON

dlBandwidth-r14 ENUMERATED {n6, n15, n25, n50, n75, n100}

OPTIONAL, -- Cond NotSameAsRef6

addPRSconfigNeighbour-r14 SEQUENCE (SIZE (1..maxAddPRSconfig-r14)) OF

Add-PRSconfigNeighbourElement-r14

OPTIONAL -- Need ON

]],

[[

tdd-config-v1520 TDD-Config-v1520 OPTIONAL -- Need ON

]]

}

Add-PRSconfigNeighbourElement-r14 ::= SEQUENCE {

add-prsInfo-r14 PRS-Info OPTIONAL, -- Cond NotSameAsRef7

...

}

maxFreqLayers INTEGER ::= 3

-- ASN1STOP

| Conditional presence | Explanation |
| --- | --- |
| *NotsameAsRef0* | The field is absent if *earfcn-v9a0* is present. If earfcn-v9a0 is not present, the field is mandatory present if the EARFCN is not the same as for the assistance data reference cell; otherwise it is not present. |
| *NotsameAsRef1* | The field is mandatory present if the cyclic prefix length is not the same as for the assistance data reference cell; otherwise it is not present. |
| *NotsameAsRef2* | The field is mandatory present if the first PRS configuration is not the same as for the assistance data reference cell; otherwise it is not present. |
| *NotsameAsRef3* | The field is mandatory present if the antenna port configuration is not the same as for the assistance data reference cell; otherwise it is not present. |
| *NotsameAsRef4* | The field is mandatory present if the slot timing is not the same as for the assistance data reference cell; otherwise it is not present. |
| *NotSameAsRef5* | The field is absent if *earfcn* is present. If *earfcn* is not present, the field is mandatory present if the EARFCN is not the same as for the assistance data reference cell; otherwise it is not present. |
| *InterFreq* | The field is optionally present, need OP, if the EARFCN is not the same as for the assistance data reference cell; otherwise it is not present. |
| *TBS* | The field is mandatory present if the *OTDOA-NeighbourCellInfoElement* is provided for a PRS-only TP; otherwise it is not present. |
| *CRS* | The field is optionally present, need ON, if *prsInfo* is present. Otherwise it is not present. |
| *NotSameAsRef6* | The field is mandatory present if PRS frequency hopping is used on this neighbour cell (TS 36.211 [16]) and if the downlink bandwidth configuration is not the same as for the assistance data reference cell; otherwise it is not present. |
| *NotSameAsRef7* | The field is mandatory present if any instance of the additional PRS configurations of *addPRSconfigNeighbour* is not the same as the corresponding instance of the additional PRS configuration of the *addPRSconfigRef* for the assistance data reference cell; otherwise it is not present. |

| *OTDOA-NeighbourCellInfoList* field descriptions |
| --- |
| ***physCellId***  This field specifies the physical cell identity of the neighbour cell, as defined in TS 36.331 [12]. |
| ***cellGlobalId***  This field specifies the ECGI, the globally unique identity of a cell in E-UTRA, of the neighbour cell, as defined in TS 36.331 [12]. The server should provide this field if it considers that it is needed to resolve any ambiguity in the cell identified by *physCellId*. |
| ***earfcn***  This field specifies the EARFCN of the neighbour cell. |
| ***cpLength***  This field specifies the cyclic prefix length of the neigbour cell PRS if PRS are present in this neighbour cell, otherwise this field specifies the cyclic prefix length of CRS in this neighbour cell. |
| ***prsInfo***  This field specifies the first PRS configuration of the neighbour cell.  When the EARFCN of the neighbour cell is the same as for the assistance data reference cell, the target device may assume that each PRS positioning occasion in the neighbour cell at least partially overlaps with a PRS positioning occasion in the assistance data reference cell where the maximum offset between the transmitted PRS positioning occasions may be assumed to not exceed half a subframe.  When the EARFCN of the neighbour cell is the same as for the assistance data reference cell, the target may assume that this cell has the same PRS periodicity (TPRS) as the assistance data reference cell. |
| ***antennaPortConfig***  This field specifies whether 1 (or 2) antenna port(s) or 4 antenna ports for cell specific reference signals are used. |
| ***slotNumberOffset***  This field specifies the slot number offset at the transmitter between this cell and the assistance data reference cell.  The *slotNumberOffset* together with the current slot number of the assistance data reference cell may be used to calculate the current slot number of this cell which may further be used to generate the CRS sequence by the target device. The offset corresponds to the number of full slots counted from the beginning of a radio frame of the assistance data reference cell to the beginning of the closest subsequent radio frame of this cell. If this field is absent, the slot timing is the same as for the assistance data reference cell. |
| ***prs-SubframeOffset***  This field specifies the offset between the first PRS subframe of the first PRS occasion group of the first PRS configuration in the assistance data reference cell on the reference carrier frequency layer and the first PRS subframe in the closest subsequent PRS occasion group of the PRS configuration with the longest PRS occasion group periodicity (NOTE 1) of this cell on the other carrier frequency layer. The value is given in number of full sub-frames. If the EARFCN is not the same as for the assistance data reference cell and the field is not present but PRS are available on this cell, the receiver shall consider the PRS subframe offset for this cell to be 0. |
| ***expectedRSTD***  If PRS is transmitted:  This field indicates the RSTD value that the target device is expected to measure between this cell and the assistance data reference cell. The *expectedRSTD* field takes into account the expected propagation time difference as well as transmit time difference of PRS positioning occasions between the two cells. The RSTD value can be negative and is calculated as (*expectedRSTD*-8192). The resolution is 3×Ts, with Ts=1/(15000\*2048) seconds.  If PRS is not transmitted:  This field indicates the RSTD value that the target device is expected to measure between this cell and the assistance data reference cell. The expectedRSTD field takes into account the expected propagation time difference as well as transmit time difference between the two cells. The RSTD value can be negative and is calculated as (expectedRSTD-8192). The resolution is 3´Ts, with Ts=1/(15000\*2048) seconds. |
| ***expectedRSTD-Uncertainty***  If PRS is transmitted:  This field indicates the uncertainty in *expectedRSTD*value***.*** The uncertainty is related to the location server′s a‑priori estimation of the target device location. The *expectedRSTD* and *expectedRSTD-Uncertainty* togetherdefine the search window for the target device.  The scale factor of the *expectedRSTD-Uncertainty* field is 3×Ts, with Ts=1/(15000\*2048) seconds.  The target device may assume that the beginning of the PRS occasion group of the PRS configuration with the longest PRS occasion group periodicity (NOTE) of the neighbour cell is received within the search window of size  [* expectedRSTD-Uncertainty*×3×Ts*,* *expectedRSTD-Uncertainty*×3×Ts] centred at  TREF *+* 1 millisecond×N +(*expectedRSTD*8192) ×3×Ts, where TREF is the reception time of the beginning of the first PRS occasion group of the first PRS configuration of the assistance data reference cell at the target device antenna connector, N = 0 when the EARFCN of the neighbour cell is equal to that of the assistance data reference cell, and N = *prs-SubframeOffset* otherwise.  If PRS is not transmitted:  This field indicates the uncertainty in *expectedRSTD*value***.*** The uncertainty is related to the location server′s a‑priori estimation of the target device location. The *expectedRSTD* and *expectedRSTD-Uncertainty* togetherdefine the search window for the target device. The scale factor of the *expectedRSTD-Uncertainty* field is 3×Ts, with Ts=1/(15000\*2048) seconds.  If Tx is the reception time of the beginning of the subframe X of the assistance data reference cell at the target device antenna connector, the target device may assume that the beginning of the closest subframe of this neighbour cell to subframe X is received within the search window of size [* expectedRSTD-Uncertainty*×3×Ts*,* *expectedRSTD-Uncertainty*×3×Ts] centred at Tx + (*expectedRSTD*8192) ×3×Ts, |
| ***tpId***  This field specifies an identity of the transmission point. This field together with the *physCellId* and/or *prsID* may be used to identify the transmission point in the case the same physical cell ID is shared by multiple transmission points. |
| ***prs-only-tp***  This field, if present, indicates that the *OTDOA-NeighbourCellInfoElement* is provided for a PRS-only TP.  For the purpose of RSTD measurements from a PRS-only TP, the target device shall not assume any other signals or physical channels are present other than PRS (TS 36.213 [28]).  For the purpose of RSTD measurements from a PRS-only TP, the target device shall use the *physCellId* only for PRS generation, and only if no PRS-ID is provided for this TP. |
| ***cpLengthCRS***  This field specifies the cyclic prefix length of this assistance data neighbour cell CRS. If this field is present, the target device may assume the CRS and PRS antenna ports of this assistance data neighbour cell are quasi co-located (as defined in TS 36.211 [16]). |
| ***sameMBSFNconfigNeighbour***  This field indicates whether the MBSFN subframe configuration of the neighbour cell is the same as the current primary cell of the target device. TRUE means the same, and FALSE means not the same. |
| ***dlBandwidth***  This field specifies the downlink bandwidth configuration of the neighbour cell, NRB in downlink, see TS 36.101 [21, table 5.6-1]. Enumerated value n6 corresponds to 6 resource blocks, n15 to 15 resource blocks and so on. |
| ***addPRSconfigNeighbour***  This field specifies the additional (second and possibly third) PRS configuration(s) of the neighbour cell. When the EARFCN of the neighbour cell is the same as for the assistance data reference cell, the target device may assume that each PRS positioning occasion in each instance of *addPRSconfigNeighbour* in the neighbour cell at least partially overlaps with a PRS positioning occasion of the same instance of *addPRSconfigRef* in the assistance data reference cell where the maximum offset between the transmitted PRS positioning occasions may be assumed to not exceed half a subframe.  When the EARFCN of the neighbour cell is the same as for the assistance data reference cell, the target may assume that each instance of *addPRSconfigNeighbour* of this cell has the same PRS periodicity (TPRS) as the corresponding instance of *addPRSconfigRef* of the assistance data reference cell. |
| ***tdd-config***  This field specifies the TDD specific physical channel configuration of the neighbour cell *earfcn*. The field should be present if this neighbour cell is a TDD cell and if the TDD UL/DL configuration for assistance data cells on this *earfcn* has not been provided in any other instance of *OTDOA-NeighbourCellInfoElement* or in IE *OTDOA-ReferenceCellInfo*, and is not the same as the target device′s current primary cell when this is a TDD cell. NOTE 2. |

NOTE 1: If this cell has more than one PRS configuration with equal longest PRS occasion group periodicity (i.e., PRS occasion group length times TPRS), the first such configuration is referenced. In order to avoid ambiguity for frequency hopping, a PRS occasion group should contain at least 2 PRS occasions with hopping between 2 narrowbands and at least 4 PRS occasions with hopping between 4 narrowbands.

NOTE 2: The target device assumes the same TDD UL/DL configuration for all TDD cells residing on same frequency band specified by *earfcn*. Therefore, the location server should include the field *tdd-config* only once for assistance data cells with the same *earfcn* in IE *OTDOA-ProvideAssistanceData*. The location server does not need to include the field *tdd-config* for any assistance data cell in IE *OTDOA-ProvideAssistanceData* with the same *earfcn* or the same TDD UL/DL configuration as the target devices′ current primary cell if this is a TDD cell.

#### – *OTDOA-ReferenceCellInfoNB*

The IE *OTDOA-ReferenceCellInfoNB* is used by the location server to provide NB-IoT assistance data reference cell information for OTDOA assistance data.

-- ASN1START

OTDOA-ReferenceCellInfoNB-r14 ::= SEQUENCE {

physCellIdNB-r14 INTEGER (0..503) OPTIONAL, -- Cond NoPRS-AD1

cellGlobalIdNB-r14 ECGI OPTIONAL, -- Cond NoPRS-AD2

carrierFreqRef-r14 CarrierFreq-NB-r14 OPTIONAL, -- Cond NotSameAsServ1

earfcn-r14 ARFCN-ValueEUTRA-r14 OPTIONAL, -- Cond Inband

eutra-NumCRS-Ports-r14 ENUMERATED {ports1-or-2, ports4}

OPTIONAL, -- Cond NoPRS-AD3

otdoa-SIB1-NB-repetitions-r14 ENUMERATED { r4, r8, r16 } OPTIONAL, -- Cond NotSameAsServ2

nprsInfo-r14 PRS-Info-NB-r14 OPTIONAL, -- Cond NPRS-Type1

...,

[[

nprsInfo-Type2-v1470 PRS-Info-NB-r14 OPTIONAL -- Cond NPRS-Type2

]],

[[ tdd-config-r15 TDD-Config-v1520 OPTIONAL -- Need ON

]]

}

-- ASN1STOP

| Conditional presence | Explanation |
| --- | --- |
| *NoPRS-AD1* | This field is mandatory present if the *OTDOA-ReferenceCellInfo* IE is not included in *OTDOA‑ProvideAssistanceData,* or if the *OTDOA-ReferenceCellInfo* IE is included in *OTDOA‑ProvideAssistanceData* and the narrowband physical layer cell identity is not the same as the physical cell identity provided in *OTDOA-ReferenceCellInfo* IE. Otherwise it is not present. |
| *NoPRS-AD2* | This field is optionally present, need ON, if the *OTDOA-ReferenceCellInfo* IE is not included in *OTDOA‑ProvideAssistanceData,* or if the *OTDOA-ReferenceCellInfo* IE is included in *OTDOA‑ProvideAssistanceData* and the global cell identity is not the same as provided in *OTDOA-ReferenceCellInfo* IE. |
| *NotSameAsServ1* | This field is mandatory present if the carrier frequency of the NB-IoT assistance data reference cell is not the same as the carrier frequency of the target devices' current serving NB-IoT cell. Otherwise it is not present. |
| *Inband* | This field is mandatory present, if the NPRS is configured within the LTE spectrum allocation (inband deployment). Otherwise it is not present. |
| *NoPRS-AD3* | This field is mandatory present if the *OTDOA-ReferenceCellInfo* IE is not included in *OTDOA‑ProvideAssistanceData* and if the NB-IoT assistance data reference cell is deployed within the LTE spectrum allocation (inband deployment)*.* Otherwise it is not present. |
| *NotSameAsServ2* | This field is mandatory present, if NPRS configuration Part B only is configured on the NB-IoT assistance data reference cell, and if the repetition number of SIB1-NB of the NB‑IoT assistance data reference cell is not the same as the repetition number of SIB1‑NB of the target devices′ current serving NB-IoT cell. Otherwise it is not present. |
| *NPRS-Type1* | The field is mandatory present if Type 1 narrowband positioning reference signals are available in the assistance data reference cell (TS 36.211 [16]); otherwise it is not present. |
| *NPRS-Type2* | The field is mandatory present if Type 2 narrowband positioning reference signals are available in the assistance data reference cell (TS 36.211 [16]); otherwise it is not present. |

| *OTDOA-ReferenceCellInfoNB* field descriptions |
| --- |
| ***physCellIdNB***  This field specifies the narrowband physical layer cell identity of the NB-IoT assistance data reference cell, as defined in TS 36.331 [12]. If this field is absent and if the *OTDOA-ReferenceCellInfo* IE is included in *OTDOA‑ProvideAssistanceData* the narrowband physical layer cell identity is the same as the *physCellId* provided in *OTDOA‑ReferenceCellInfo* IE. |
| ***cellGlobalIdNB***  This field specifies the global cell identity of the NB-IoT assistance data reference cell, as defined in TS 36.331 [12]. If this field is absent and if the *OTDOA-ReferenceCellInfo* IE with *cellGlobalId* is included in *OTDOA‑ProvideAssistanceData,* the global cell identity is the same as provided in *OTDOA‑ReferenceCellInfo* IE*.* |
| ***carrierFreqRef***  This field specifies the carrier frequency of the NB-IoT assistance data reference cell. |
| ***earfcn***  This field specifies the EARFCN of the E-UTRAN frequency, in which the NB-IoT cell is deployed. |
| ***eutra-NumCRS-Ports***  This field specifies whether 1 (or 2) antenna port(s) or 4 antenna ports for cell specific reference signals (CRS) are used in the NB-IoT assistance data reference cell. If this field is absent and if the *OTDOA-ReferenceCellInfo* IE is included in *OTDOA‑ProvideAssistanceData*, the number of CRS antenna ports is the same as provided in *OTDOA‑ReferenceCellInfo* IE. |
| ***otdoa-SIB1-NB-repetitions***  This field specifies the repetition number of SIB1-NB of the NB-IoT assistance data reference cell. Enumerated values r4 correspond to 4 repetions, r8 to 8 repetitions, and r16 to 16 repetions.  Note, when NPRS configuration Part B only is configured on the NB-IoT assistance data reference cell (i.e., anchor carrier), *nprs-NumSF* does also count/include subframes containing NPSS, NSSS, NPBCH, or SIB1-NB, but the UE can assume that no NPRS are transmitted in these subframes (TS 36.211 [16]). |
| ***nprsInfo***  This field specifies the Type 1 NPRS (TS 36.211 [16]) configuration of the NB-IoT assistance data reference cell.  When the target device receives this field with *operationModeInfoNPRS* set to value ′*standalone*′, the target device shall assume no NPRS are transmitted on that NB-IoT carrier. |
| ***nprsInfo-Type2***  This field specifies the Type 2 NPRS (TS 36.211 [16]) configuration of the NB-IoT assistance data reference cell. |
| ***tdd-config***  Indicates the TDD specific physical channel configuration of the NB-IoT assistance data reference cell operating in TDD mode. This field should be present if the DL/UL subframe configuration of the NB-IoT assistance data reference cell is not the same as the DL/UL subframe configuration of the current serving NB-IoT cell of the target device, or if the current serving NB-IoT cell of the target device operates in FDD mode. |

#### – *PRS-Info-NB*

The IE *PRS-Info-NB* provides the information related to the configuration of NPRS in a cell. If *PRS-Info-NB* includes configurations for multiple NPRS carrier frequencies, the target device may assume the antenna ports for the NPRS carrier are quasi co-located, as defined in TS 36.211 [16].

-- ASN1START

PRS-Info-NB-r14 ::= SEQUENCE (SIZE (1..maxCarrier-r14)) OF NPRS-Info-r14

NPRS-Info-r14 ::= SEQUENCE {

operationModeInfoNPRS-r14 ENUMERATED { inband, standalone },

nprs-carrier-r14 CarrierFreq-NB-r14 OPTIONAL, -- Cond Standalone/Guardband

nprsSequenceInfo-r14 INTEGER (0..174) OPTIONAL, -- Cond Inband

nprsID-r14 INTEGER (0..4095) OPTIONAL, -- Cond NPRS-ID

partA-r14 SEQUENCE {

nprsBitmap-r14 CHOICE {

subframePattern10-r14 BIT STRING (SIZE (10)),

subframePattern40-r14 BIT STRING (SIZE (40))

},

nprs-MutingInfoA-r14 CHOICE {

po2-r14 BIT STRING (SIZE(2)),

po4-r14 BIT STRING (SIZE(4)),

po8-r14 BIT STRING (SIZE(8)),

po16-r14 BIT STRING (SIZE(16)),

...

} OPTIONAL, -- Cond MutingA

...

} OPTIONAL, -- Cond PartA

partB-r14 SEQUENCE {

nprs-Period-r14 ENUMERATED { ms160, ms320, ms640, ms1280, ... , ms2560-v1510},

nprs-startSF-r14 ENUMERATED { zero, one-eighth, two-eighths, three-eighths,

four-eighths, five-eighths, six-eighths,

seven-eighths, ...},

nprs-NumSF-r14 ENUMERATED { sf10, sf20, sf40, sf80, sf160, sf320,

sf640, sf1280, ... , sf2560-v1510},

nprs-MutingInfoB-r14 CHOICE {

po2-r14 BIT STRING (SIZE(2)),

po4-r14 BIT STRING (SIZE(4)),

po8-r14 BIT STRING (SIZE(8)),

po16-r14 BIT STRING (SIZE(16)),

...

} OPTIONAL, -- Cond MutingB

...,

[[ sib1-SF-TDD-r15 ENUMERATED {sf0, sf4, sf0and5} OPTIONAL -- Cond SIB1-TDD

]]

} OPTIONAL, -- Cond PartB

...,

[[

partA-TDD-r15 SEQUENCE {

nprsBitmap-r15 CHOICE {

subframePattern10-TDD-r15 BIT STRING (SIZE (8)),

subframePattern40-TDD-r15 BIT STRING (SIZE (32)),

...

},

nprs-MutingInfoA-r15 CHOICE {

po2-r15 BIT STRING (SIZE(2)),

po4-r15 BIT STRING (SIZE(4)),

po8-r15 BIT STRING (SIZE(8)),

po16-r15 BIT STRING (SIZE(16)),

...

} OPTIONAL, -- Cond MutingA

...

} OPTIONAL -- Cond PartA-TDD

]]

}

maxCarrier-r14 INTEGER ::= 5

-- ASN1STOP

| Conditional presence | Explanation |
| --- | --- |
| *Standalone/Guardband* | This field is mandatory present, if the NPRS is configured in standalone or guardband operation mode. Otherwise it is not present. |
| *Inband* | This field is mandatory present, if the NPRS is configured within the LTE spectrum allocation (inband deployment) and the LTE carrier frequency is not provided in the assistance data. Otherwise it is not present. |
| *NPRS-ID* | The field is mandatory present, if the NPRS is generated based on the NPRS-ID (TS 36.211 [16]), different from the PCI. Otherwise the field is not present. |
| *MutingA* | The field is mandatory present, if muting is used for the NPRS Part A or Part A TDD configuration. Otherwise the field is not present. |
| *PartA* | The field is mandatory present, if NPRS is configured based on a bitmap of subframes which are not NB-IoT DL subframes (i.e., invalid DL subframes) (Part A configuration). Otherwise the field is not present. This field is not applicable for NB-IoT operating in TDD mode. |
| *MutingB* | The field is mandatory present, if muting is used for the NPRS Part B configuration. Otherwise the field is not present. |
| *PartB* | The field is mandatory present, if NPRS is configured based on a NPRS period, a NPRS subframe offset, and a number of consecutive NPRS downlink subframes per positioning occasion (Part B configuration). Otherwise the field is not present.  If NPRS configuration Part A and Part B are both configured, then a subframe contains NPRS if both configurations indicate that it contains NPRS. |
| *PartA-TDD* | The field is mandatory present, if NPRS is configured for NB-IoT operating in TDD mode and if NPRS is configured based on a bitmap of subframes which are not NB-IoT DL subframes (i.e., invalid DL subframes) (Part A TDD configuration). Otherwise the field is not present. |
| *SIB1-TDD* | The field is mandatory present, if NPRS is configured for NB-IoT operating in TDD mode and if SIB1-NB is transmitted on this carrier frequency. Otherwise the field is not present. |

| *PRS-Info-NB* field descriptions |
| --- |
| ***operationModeInfoNPRS***  This field specifies the operation mode of the NPRS carrier. The value ′standalone′ indicates standalone or guardband operation mode. |
| ***nprs-carrier***  This field specifies the NB-IoT carrier frequency for the NPRS. |
| ***nprsSequenceInfo***  This field specifies the index of the PRB containing the NPRS as defined in the table *nprsSequenceInfo* to E‑UTRA PRB index relation below. |
| ***nprsID***  This field specifies the NPRS-ID as defined in TS 36.211 [16]. |
| ***sib1-SF-TDD***  This field indicates the subframe(s) used to transmit SIB1-NB. Values *sf0* and *sf4* correspond with subframe #0 and #4 respectively. Value *sf0and5* corresponds with subframes #0 and #5. |
| ***subframePattern10, subframePattern40***  This field specifies the NPRS subframe Part A configuration over 10 ms or 40 ms. Subframes not containing NPRS are indicated with value ′0′ in the bitmap; subframes containing NPRS are indicated with value ′1′ in the bitmap. The first/leftmost bit corresponds to the subframe #0 of the radio frame satisfying SFN mod x = 0, where x is the size of the bit string divided by 10. |
| ***nprs-MutingInfoA***  This field specifies the NPRS muting configuration of the NB-IoT carrier Part A configuration. The NPRS muting configuration is defined by a periodic NPRS muting sequence with periodicity TREP where TREP, counted in the number of NPRS positioning occasions, can be 2, 4, 8, or 16 which is also the length of the selected bit string that represents this NPRS muting sequence. If a bit in the NPRS muting sequence is set to ′0′, then the NPRS is muted in the corresponding NPRS positioning occasion. A NPRS positioning occasion for Part A comprises one radio frame (i.e., 10 subframes). The first/leftmost bit of the NPRS muting sequence corresponds to the first NPRS positioning occasion that starts after the beginning of the NB-IoT assistance data reference cell SFN=0. The sequence is valid for all subframes after the target device has received the *nprs-MutingInfoA*.  When the SFN of the NB-IoT assistance data reference cell is not known to the target device and *nprs-MutingInfoA* is provided for a cell in the *OTDOA-NeighbourCellInfoListNB* IE, the target device may assume no NPRS is transmitted by that cell. |
| ***nprs-Period***  This field specifies the NPRS occasion period *TNPRS*(TS 36.211 [16]). Enumerated values correspond to 160 ms, 320 ms, 640 ms, 1280 ms, and 2560 ms. The value *ms2560* is only applicable to TDD mode. |
| ***nprs-startSF***  This field specifies the subframe offset (TS 36.211[16]). Enumerated values correspond to  of 0, 1/8, 2/8, 3/8, 4/8, 5/8, 6/8, or 7/8. |
| ***nprs-NumSF***  This field specifies the number of consecutive downlink subframes NNPRS in one NPRS positioning occasion (TS 36.211 [16]). Enumerated values correspond to 10, 20, 40, 80, 160, 320, 640, 1280, and 2560 subframes. The values *sf10* and *sf20* are only applicable to FDD mode. The value *sf2560* is only applicable to TDD mode.  When the target device receives a *nprs-NumSF* which exceeds the *nprs-Period* (i.e., *NNPRS* > *TNPRS*), the target device may assume no NPRS is transmitted by that cell. |
| ***nprs-MutingInfoB***  This field specifies the NPRS muting configuration of the NB-IoT carrier Part B configuration. The NPRS muting configuration is defined by a periodic NPRS muting sequence with periodicity TREP where TREP, counted in the number of NPRS positioning occasions, can be 2, 4, 8, or 16 which is also the length of the selected bit string that represents this NPRS muting sequence. If a bit in the NPRS muting sequence is set to ′0′, then the NPRS is muted in the corresponding NPRS positioning occasion. A NPRS positioning occasion for Part B comprises NNPRS consecutive downlink positioning subframes, where NNPRS is given by the *nprs-NumSF* field. The first/leftmost bit of the NPRS muting sequence corresponds to the first NPRS positioning occasion that starts after the beginning of the NB-IoT assistance data reference cell SFN=0. The sequence is valid for all subframes after the target device has received the *nprs‑MutingInfoB*.  When the SFN of the NB-IoT assistance data reference cell is not known to the UE and *nprs-MutingInfoB* is provided for a cell in the *OTDOA-NeighbourCellInfoListNB* IE, the target device may assume no NPRS is transmitted by that cell.  When the UE receives a TREP-bit muting pattern together with a NPRS periodicity TNPRS for the same carrier which exceeds 10240 subframes (i.e., TREP × TNPRS > 10240 subframes), the target device shall assume an n-bit muting pattern based on the first n bits, where n = 10240/TNPRS. |
| ***subframePattern10-TDD, subframePattern40-TDD***  This field specifies the NPRS subframe Part A configuration for TDD over 10 ms or 40 ms. The UE shall assume that subframe number 1 and 2 are not used for NPRS. The MSB of the NPRS bitmap corresponds to subframe 0, the second MSB corresponds to subframe 3, the third MSB corresponds to subframe 4 and so on, as also shown in Figure NPRS bitmap to subframe number mapping below. |

*nprsSequenceInfo* to E‑UTRA PRB index relation

|  |  |  |  |
| --- | --- | --- | --- |
| *nprsSequenceInfo* | E-UTRA PRB index for odd number of [16] | *nprsSequenceInfo* | E-UTRA PRB index for even number of [16] |
| 0 - 74 | -37, -36, …, 37 | 75 – 174 | -50, -49, …, 49 |

NOTE: Based on the above relation, in inband deployment, the carrier frequency of the NPRS carrier (*f*NB-IoT) can be calculated as follows:

where *f*EUTRA isderived from *earfcn* according to TS 36.101 [21, 5.7.3].



Figure 6.5.1.2-1: NPRS bitmap to subframe number mapping

#### – *OTDOA-NeighbourCellInfoListNB*

The IE *OTDOA-NeighbourCellInfoListNB* is used by the location server to provide NB-IoT neighbour cell information for OTDOA assistance data.

-- ASN1START

OTDOA-NeighbourCellInfoListNB-r14 ::= SEQUENCE (SIZE (1..maxCells-r14)) OF

OTDOA-NeighbourCellInfoNB-r14

OTDOA-NeighbourCellInfoNB-r14 ::= SEQUENCE {

physCellIdNB-r14 INTEGER (0..503) OPTIONAL, -- Cond NoPRS-AD1

cellGlobalIdNB-r14 ECGI OPTIONAL, -- Cond NoPRS-AD2

carrierFreq-r14 CarrierFreq-NB-r14 OPTIONAL, -- Cond NotSameAsRef1

earfcn-r14 ARFCN-ValueEUTRA-r14 OPTIONAL, -- Cond Inband

eutra-NumCRS-Ports-r14 ENUMERATED {ports-1-or-2, ports-4, ...}

OPTIONAL, -- Cond NotsameAsRef2

otdoa-SIB1-NB-repetitions-r14 ENUMERATED { r4, r8, r16 }

OPTIONAL, -- Cond NotSameAsRef3

nprsInfo-r14 PRS-Info-NB-r14 OPTIONAL, -- Cond NotsameAsRef4

nprs-slotNumberOffset-r14 INTEGER (0..19) OPTIONAL, -- Cond NotsameAsRef5

nprs-SFN-Offset-r14 INTEGER (0..63) OPTIONAL, -- Cond NotsameAsRef6

nprs-SubframeOffset-r14 INTEGER (0..1279) OPTIONAL, -- Need OP

expectedRSTD-r14 INTEGER (0..16383) OPTIONAL, -- Cond NoPRS-AD3

expectedRSTD-Uncertainty-r14 INTEGER (0..1023) OPTIONAL, -- Cond NoPRS-AD3

prsNeighbourCellIndex-r14 INTEGER (1..72) OPTIONAL, -- Cond PRS-AD

...,

[[

nprsInfo-Type2-v1470 PRS-Info-NB-r14 OPTIONAL -- Cond NotSameAsRef4

]],

[[ tdd-config-r15 TDD-Config-v1520 OPTIONAL -- Need ON

]]

}

maxCells-r14 INTEGER ::= 72

-- ASN1STOP

| Conditional presence | Explanation |
| --- | --- |
| *NoPRS-AD1* | This field is mandatory present if the *OTDOA-NeighbourCellInfoList* IE is not included in *OTDOA‑ProvideAssistanceData,* or if the *OTDOA-NeighbourCellInfoList* IE is included in *OTDOA‑ProvideAssistanceData* and the narrowband physical layer cell identity of this cell is not the same as the physical cell identity of the corresponding cell (as indicated by *prsNeighbourCellIndex*) in *OTDOA‑NeighbourCellInfoList* IE. |
| *NoPRS-AD2* | This field is optionally present, need ON, if the *OTDOA-NeighbourCellInfoList* IE is not included in *OTDOA‑ProvideAssistanceData,* or if the *OTDOA-NeighbourCellInfoList* IE is included in *OTDOA‑ProvideAssistanceData* and the global cell identity of this cell is not the same as for the corresponding cell (as indicated by *prsNeighbourCellIndex*) in *OTDOA‑NeighbourCellInfoList* IE. |
| *Inband* | This field is mandatory present, if the NPRS is configured within the LTE spectrum allocation (inband deployment). Otherwise it is not present. |
| *NotSameAsRef1* | The field is mandatory present if the carrier frequency is not the same as for the NB-IoT assistance data reference cell; otherwise it is not present. |
| *NotSameAsRef2* | The field is mandatory present if this cell is deployed within the LTE spectrum allocation (inband deployment) and if the number of E-UTRA CRS antenna ports is not the same as for the NB-IoT assistance data reference cell; otherwise it is not present. |
| *NotSameAsRef3* | This field is mandatory present if NPRS configuration Part B only is configured on this neighbour cell, and if the repetition number of SIB1-NB of this neighbor cell is not the same as the repetition number of SIB1‑NB of the NB-IoT assistance data reference cell. Otherwise it is not present. |
| *NotSameAsRef4* | The field is mandatory present, if the NPRS configuration is not the same as for the NB‑IoT assistance data reference cell; otherwise it is not present. |
| *NotSameAsRef5* | The field is mandatory present if the slot timing is not the same as for the NB-IoT assistance data reference cell; otherwise it is not present. |
| *NotSameAsRef6* | The field is mandatory present if the frame timing is not the same as for the NB-IoT assistance data reference cell; otherwise it is not present. |
| *NoPRS-AD3* | This field is mandatory present if the *OTDOA-NeighbourCellInfoList* IE is not included in *OTDOA‑ProvideAssistanceData,* or if the *OTDOA-NeighbourCellInfoList* IE is included in *OTDOA‑ProvideAssistanceData* and *prsNeighbourCellIndex* is absent for this cell. |
| *PRS-AD* | This field is optionally present, need OP, if the *OTDOA-NeighbourCellInfoList* IE is included in *OTDOA‑ProvideAssistanceData*; otherwise it is not present. |

| *OTDOA-NeighbourCellInfoListNB* field descriptions |
| --- |
| ***physCellIdNB***  This field specifies the narrowband physical cell identity of the NB-IoT neighbour cell, as defined in TS 36.331 [12]. If this field is absent and if the *OTDOA-NeighbourCellInfoList* IE is included in *OTDOA‑ProvideAssistanceData* the narrowband physical layer cell identity is the same as the *physCellId* provided for the corresponding cell (as indicated by *prsNeighbourCellIndex*) in *OTDOA‑NeighbourCellInfoList* IE. |
| ***cellGlobalIdNB***  This field specifies the global cell ID of the NB-IoT neighbour cell, as defined in TS 36.331 [12]. If this field is absent and if the *OTDOA‑NeighbourCellInfoList* IE with *cellGlobalId* is included in *OTDOA‑ProvideAssistanceData,* the global cell identity of the NB-IoT neighbour cell is the same as provided for the corresponding cell (as indicated by *prsNeighbourCellIndex*) in *OTDOA‑NeighbourCellInfoList* IE*.* |
| ***carrierFreq***  This field specifies the carrier frequency of the NB-IoT neighbour cell. |
| ***earfcn***  This field specifies the EARFCN of the E-UTRAN frequency, in which the NB-IoT cell is deployed. |
| ***eutra-NumCRS-Ports***  This field specifies whether 1 (or 2) antenna port(s) or 4 antenna ports for cell specific reference signals are used. |
| ***otdoa-SIB1-NB-repetitions***  This field specifies the repetition number of SIB1-NB of the neighbour cell. Enumerated values r4 correspond to 4 repetions, r8 to 8 repetitions, and r16 to 16 repetions.  Note, when NPRS configuration Part B only is configured on this NB-IoT neighbour cell (i.e., anchor carrier), *nprs-NumSF* does also count/include subframes containing NPSS, NSSS, NPBCH, or SIB1-NB, but the UE can assume that no NPRS are transmitted in these subframes (TS 36.211 [16]). |
| ***nprsInfo***  This field specifies the Type 1 NPRS (TS 36.211 [16]) configuration of the NB-IoT neighbour cell.  When the carrier frequency of the NB-IoT neighbour cell is the same as for the NB-IoT assistance data reference cell, the target device may assume that each NPRS positioning occasion for each NPRS carrier frequency in the neighbour cell at least partially overlaps with a NPRS positioning occasion for each NPRS carrier frequency in the NB-IoT assistance data reference cell where the maximum offset between the transmitted NPRS positioning occasions may be assumed to not exceed half a subframe.  When the carrier frequency of the neighbour cell is the same as for the NB-IoT assistance data reference cell, and NPRS configuration Part B is configured, the target may assume that this cell has the same NPRS periodicity (TNPRS) as the assistance data reference cell for each NPRS carrier frequency.  When the target device receives this field with *operationModeInfoNPRS* set to value ′*standalone*′, the target device shall assume no NPRS are transmitted on that NB-IoT carrier. |
| ***nprs-slotNumberOffset***  This field specifies the slot number offset at the transmitter between this cell and the NB-IoT assistance data reference cell. The offset corresponds to the number of full slots counted from the beginning of a radio frame of the NB-IoT assistance data reference cell to the beginning of the closest subsequent radio frame of this cell. If this field is absent, the slot timing is the same as for the NB-IoT assistance data reference cell. |
| ***nprs-SFN-Offset***  This field specifies the SFN offset (modulo 64) at the transmitter between this cell and the NB-IoT assistance data reference cell. The offset corresponds to the number of full radio frames counted from the beginning of a radio frame #0 of the NB‑IoT assistance data reference cell to the beginning of the closest subsequent radio frame #0 of this cell.  The UE may use this field together with the *nprs-slotNumberOffset* and *otdoa-SIB1-NB-repetitions* to determine the SIB1-NB subframes of this neighbour cell. |
| ***nprs-SubframeOffset***  This field specifies the offset between the first NPRS subframe in the NB-IoT assistance data reference cell (NOTE 1) and the first NPRS subframe in the closest subsequent NPRS positioning occasion of the NPRS carrier with the longest NPRS periodicity of this cell (NOTE 2). The value is given in number of full sub-frames. If this field is not present, the receiver shall consider the NPRS subframe offset to be 0. |
| ***expectedRSTD***  This field indicates the RSTD value that the target device is expected to measure between this cell and the NB-IoT assistance data reference cell. The *expectedRSTD* field takes into account the expected propagation time difference as well as transmit time difference of NPRS positioning occasions between the two cells. The RSTD value can be negative and is calculated as (*expectedRSTD*-8192). The resolution is 3×Ts, with Ts=1/(15000\*2048) seconds.  If this field is absent and if the *OTDOA-NeighbourCellInfoList* IE is included in *OTDOA‑ProvideAssistanceData*, the expected RSTD is the same as provided in *OTDOA-NeighbourCellInfoList* IE for the corresponding cell (as indicated by *prsNeighbourCellIndex*). |
| ***expectedRSTD-Uncertainty***  This field indicates the uncertainty in *expectedRSTD*value***.*** The uncertainty is related to the location server′s a‑priori estimation of the target device location. The *expectedRSTD* and *expectedRSTD-Uncertainty* togetherdefine the search window for the target device.  The scale factor of the *expectedRSTD-Uncertainty* field is 3×Ts, with Ts=1/(15000\*2048) seconds.  If this field is absent and if the *OTDOA-NeighbourCellInfoList* IE is included in *OTDOA‑ProvideAssistanceData*, the expected RSTD uncertainty is the same as provided in *OTDOA-NeighbourCellInfoList* IE for the corresponding cell (as indicated by *prsNeighbourCellIndex*).  The target device may assume that the beginning of the NPRS positioning occasion of the NPRS carrier with the longest NPRS periodicity of the neighbour cell (NOTE 2) is received within the search window of size [*expectedRSTD-Uncertainty*×3×Ts*,* *expectedRSTD-Uncertainty*×3×Ts] centred at  TREF *+* 1 millisecond×N +(*expectedRSTD*8192) ×3×Ts, where TREF is the reception time of the beginning of the NPRS positioning occasion of the NB-IoT assistance data reference cell (NOTE 1) at the target device antenna connector, and N = *nprs‑SubframeOffset*. |
| ***prsNeighbourCellIndex***  This field contains an index of the entry in IE *OTDOA-NeighbourCellInfoList*. Value 1 corresponds to the first cell in *OTDOA-NeighbourCellInfoList,* value 2 to the second, and so on. If this field is absent, and if the *OTDOA‑NeighbourCellInfoList* IE is included in *OTDOA‑ProvideAssistanceData,* it means there is no corresponding cell in *OTDOA-NeighbourCellInfoList* IE for this cell.  The target device may assume the antenna ports of the PRS of the cell indicated by *prsNeighbourCellIndex*and the NPRS of this cell are quasi co-located, as defined in TS 36.211 [16]. |
| ***nprsInfo-Type2***  This field specifies the Type 2 NPRS (TS 36.211 [16]) configuration of the NB-IoT neighbour cell. |
| ***tdd-config***  Indicates the TDD specific physical channel configuration of the NB-IoT assistance data neighbour cell operating in TDD mode. This field should be present if the DL/UL subframe configuration of the NB-IoT assistance data neighbour cell is not the same as for the NB-IoT assistance data reference cell, or if the current serving NB-IoT cell of the target device operates in FDD mode. |

NOTE 1: If the NB-IoT assistance data reference cell (i.e., anchor carrier) has no NPRS configured, the first NPRS carrier in *PRS-Info-NB* is referenced.

NOTE 2: "Cell" in this context may not necessarily be the anchor carrier. If this "cell" has more than one NPRS carrier with equal longest periodicity, the first such NPRS carrier in *PRS-Info-NB* is referenced. The length of a NPRS positioning occasion for Part A in this context is the length of the *nprsBitmap* bit string.

#### 6.5.1.3 OTDOA Assistance Data Request

#### – *OTDOA-RequestAssistanceData*

The IE *OTDOA-RequestAssistanceData* is used by the target device to request assistance data from a location server.

-- ASN1START

OTDOA-RequestAssistanceData ::= SEQUENCE {

physCellId INTEGER (0..503),

...,

[[

adType-r14 BIT STRING { prs (0), nprs (1) } (SIZE (1..8)) OPTIONAL

]],

[[

nrPhysCellId-r15 INTEGER (0..1007) OPTIONAL

]]

}

-- ASN1STOP

| *OTDOA-RequestAssistanceData* field descriptions |
| --- |
| ***physCellId***  This field specifies the E-UTRA physical cell identity of the current primary cell of the target device. |
| ***adType***  This field specifies the assistance data requested. This is represented by a bit string, with a one-value at the bit position means the particular assistance data is requested; a zero-value means not requested.  Bit 0 indicates that PRS assistance data are requested, bit 1 indicates that NPRS assistance data are requested. |
| ***nrPhysCellId***  This field specifies the NR physical cell identity of the current primary cell of the target device. If this field is present, the target device sets the *physCellId* to an arbitrary value which shall be ignored by the location server. |

#### 6.5.1.4 OTDOA Location Information

#### – *OTDOA-ProvideLocationInformation*

The IE *OTDOA-ProvideLocationInformation* is used by the target device to provide OTDOA location measurements to the location server. It may also be used to provide OTDOA positioning specific error reason.

-- ASN1START

OTDOA-ProvideLocationInformation ::= SEQUENCE {

otdoaSignalMeasurementInformation OTDOA-SignalMeasurementInformation OPTIONAL,

otdoa-Error OTDOA-Error OPTIONAL,

...,

[[

otdoaSignalMeasurementInformation-NB-r14 OTDOA-SignalMeasurementInformation-NB-r14

OPTIONAL

]]

}

-- ASN1STOP

#### 6.5.1.5 OTDOA Location Information Elements

#### – *OTDOA-SignalMeasurementInformation*

The IE *OTDOA-SignalMeasurementInformation* is used by the target device to provide RSTD measurements to the location server. The RSTD measurements are provided for a neighbour cell and the RSTD reference cell, both of which are provided in the IE *OTDOA-ProvideAssistanceData.* The RSTD reference cell may or may not be the same as the assistance data reference cell provided in *OTDOA-ReferenceCellInfo* or *OTDOA-ReferenceCellInfoNB*. If the target device stops reporting inter-frequency RSTD measurements, where the inter-frequency RSTD measurement is an OTDOA RSTD measurement with at least one cell on a frequency different from the serving cell frequency, the LPP layer shall inform lower layers that inter-frequency RSTD measurements are stopped.

NOTE 1: If there are more than 24 *NeighbourMeasurementElement* to be sent, the target device may send them in multiple *ProvideLocationInformation* messages, as described under clause 5.3.

NOTE 2: If NPRS/PRS antenna ports are quasi co-located, the target device provides a single RSTD measurement for the quasi co-located antenna ports of NPRS/PRS.

-- ASN1START

OTDOA-SignalMeasurementInformation ::= SEQUENCE {

systemFrameNumber BIT STRING (SIZE (10)),

physCellIdRef INTEGER (0..503),

cellGlobalIdRef ECGI OPTIONAL,

earfcnRef ARFCN-ValueEUTRA OPTIONAL, -- Cond NotSameAsRef0

referenceQuality OTDOA-MeasQuality OPTIONAL,

neighbourMeasurementList NeighbourMeasurementList,

...,

[[ earfcnRef-v9a0 ARFCN-ValueEUTRA-v9a0 OPTIONAL -- Cond NotSameAsRef1

]],

[[ tpIdRef-r14 INTEGER (0..4095) OPTIONAL, -- Cond ProvidedByServer0

prsIdRef-r14 INTEGER (0..4095) OPTIONAL, -- Cond ProvidedByServer1

additionalPathsRef-r14

AdditionalPathList-r14 OPTIONAL,

nprsIdRef-r14 INTEGER (0..4095) OPTIONAL, -- Cond ProvidedByServer2

carrierFreqOffsetNB-Ref-r14

CarrierFreqOffsetNB-r14 OPTIONAL, -- Cond NB-IoT

hyperSFN-r14 BIT STRING (SIZE (10)) OPTIONAL -- Cond H-SFN

]],

[[

motionTimeSource-r15 MotionTimeSource-r15 OPTIONAL

]]

}

NeighbourMeasurementList ::= SEQUENCE (SIZE(1..24)) OF NeighbourMeasurementElement

NeighbourMeasurementElement ::= SEQUENCE {

physCellIdNeighbour INTEGER (0..503),

cellGlobalIdNeighbour ECGI OPTIONAL,

earfcnNeighbour ARFCN-ValueEUTRA OPTIONAL, -- Cond NotSameAsRef2

rstd INTEGER (0..12711),

rstd-Quality OTDOA-MeasQuality,

...,

[[ earfcnNeighbour-v9a0 ARFCN-ValueEUTRA-v9a0 OPTIONAL -- Cond NotSameAsRef3

]],

[[ tpIdNeighbour-r14 INTEGER (0..4095) OPTIONAL, -- Cond ProvidedByServer0

prsIdNeighbour-r14 INTEGER (0..4095) OPTIONAL, -- Cond ProvidedByServer1

delta-rstd-r14 INTEGER (0..5) OPTIONAL,

additionalPathsNeighbour-r14

AdditionalPathList-r14 OPTIONAL,

nprsIdNeighbour-r14 INTEGER (0..4095) OPTIONAL, -- Cond ProvidedByServer2

carrierFreqOffsetNB-Neighbour-r14 CarrierFreqOffsetNB-r14 OPTIONAL -- Cond NB-IoT

]],

[[

delta-SFN-r15 INTEGER (-8192..8191) OPTIONAL

]]

}

AdditionalPathList-r14 ::= SEQUENCE (SIZE(1..maxPaths-r14)) OF AdditionalPath-r14

maxPaths-r14 INTEGER ::= 2

MotionTimeSource-r15 ::= SEQUENCE {

timeSource-r15 ENUMERATED {servingCell, referenceCell, gnss, mixed,

other, none, ...}

}

-- ASN1STOP

| Conditional presence | Explanation |
| --- | --- |
| *NotSameAsRef0* | The field is absent if the corresponding *earfcnRef-v9a0* is present. Otherwise, the target device shall include this field if the EARFCN of the RSTD reference cell is not the same as the EARFCN of the assistance data reference cell provided in the OTDOA assistance data. |
| *NotSameAsRef1* | The field is absent if the corresponding *earfcnRef* is present. Otherwise, the target device shall include this field if the EARFCN of the RSTD reference cell is not the same as the EARFCN of the assistance data reference cell provided in the OTDOA assistance data. |
| *NotSameAsRef2* | The field is absent if the corresponding *earfcnNeighbour-v9a0* is present. Otherwise, the target device shall include this field if the EARFCN of this neighbour cell is not the same as the *earfcnRef*for the RSTD reference cell. |
| *NotSameAsRef3* | The field is absent if the corresponding *earfcnNeighbour* is present. Otherwise, the target device shall include this field if the EARFCN of this neighbour cell is not the same as the *earfcnRef*for the RSTD reference cell. |
| *ProvidedByServer0* | The target device shall include this field if a *tpId* for this transmission point is included in the *OTDOA-ProvideAssistanceData.* Otherwise the field is absent. |
| *ProvidedByServer1* | The target device shall include this field if a *prsID* for this transmission point is included in the *OTDOA-ProvideAssistanceData.* Otherwise the field is absent. |
| *ProvidedByServer2* | The target device shall include this field if an *nprsID* for this cell is included in the *OTDOA-ProvideAssistanceData* and if this cell is a NB-IoT only cell (without associated LTE PRS cell)*.* Otherwise the field is absent. |
| *NB-IoT* | The target device shall include this field if the cell is a NB-IoT only cell (without associated LTE PRS cell). Otherwise the field is absent. |
| *H-SFN* | The target device shall include this field if it was able to determine a hyper SFN of the RSTD reference cell. |

| *OTDOA-SignalMeasurementInformation* field descriptions |
| --- |
| ***systemFrameNumber***  If the *delta-SFN* and *motionTimeSource* fields are not present, this field specifies the SFN of the RSTD reference cell containing the starting subframe of the PRS or NPRS positioning occasion if PRS or NPRS are available on the RSTD reference cell, or subframe of the CRS for RSTD measurements if PRS and NPRS are not available on the RSTD reference cell during which the most recent neighbour cell RSTD measurement was performed.  In the case of more than a single PRS configuration on the RSTD reference cell, the first PRS configuration is referenced.  If the *delta-SFN* and *motionTimeSource* fields are present, this field specifies the SFN of the RSTD reference cell when the TOA measurement for the RSTD reference cell has been made. |
| ***physCellIdRef***  This field specifies the physical cell identity of the RSTD reference cell. |
| ***cellGlobalIdRef***  This field specifies the ECGI, the globally unique identity of a cell in E-UTRA, of the RSTD reference cell. The target shall provide this IE if it knows the ECGI of the RSTD reference cell. |
| ***earfcnRef***  This field specifies the EARFCN of the RSTD reference cell. |
| ***referenceQuality***  This field specifies the target device′s best estimate of the quality of the TOA measurement from the RSTD reference cell, TSubframeRxRef, where TSubframeRxRef is the time of arrival of the signal from the RSTD reference cell.  When *delta-SFN* and *motionTimeSource* are both included, the target device shall not include measurement errors caused by motion of the target device in *referenceQuality* (e.g. the target device may assume the target device was stationary during OTDOA measurements). |
| ***neighbourMeasurementList***  This list contains the measured RSTD values for neighbour cells together with the RSTD reference cell, along with quality for each measurement. |
| ***tpIdRef***  This field specifies the transmission point ID of the RSTD reference cell. |
| ***prsIdRef***  This field specifies the PRS-ID of the first PRS configuration of the RSTD reference cell. |
| ***additionalPathsRef***  This field specifies one or more additional detected path timing values for the RSTD reference cell, relative to the path timing used for determining the *rstd* value. If this field was requested but is not included, it means the UE did not detect any additional path timing values. |
| ***nprsIdRef***  This field specifies the NPRS-ID of the RSTD reference cell. |
| ***carrierFreqOffsetNB-Ref***  This field specifies the offset of the NB-IoT channel number to EARFCN given by *earfcnRef* as defined in TS 36.101 [21]. |
| ***hyperSFN***  This field specifies the hyper SFN as defined in TS 36.331 [12] of the RSTD reference cell for the *systemFrameNumber*. |
| ***motionTimeSource***  This field provides reference information concerning the movement of the target device and comprises the following subfields:  - ***timeSource*** specifies the external time source to which UE time was locked during the OTDOA measurements. Enumerated value "mixed" indicates that UE time was locked to more than one external time source during OTDOA measurements (e.g. is applicable to a change in serving cell when the serving cell was used as a time source). The value "other" indicates some other external time source. The value "none" indicates that UE time was not locked to an external time source.  If this field is present, the target device shall also provide the IE *Sensor-MotionInformation* in IE *Sensor‑ProvideLocationInformation*. |
| ***physCellIdNeighbour***  This field specifies the physical cell identity of the neighbour cell for which the RSTDs are provided. |
| ***cellGlobalIdNeighbour***  This field specifies the ECGI, the globally unique identity of a cell in E-UTRA, of the neighbour cell for which the RSTDs are provided. The target device shall provide this IE if it was able to determine the ECGI of the neighbour cell at the time of measurement. |
| ***earfcnNeighbour***  This field specifies the EARFCN of the neighbour cell used for the RSTD measurements. |
| ***rstd***  This field specifies the relative timing difference between this neighbour cell and the RSTD reference cell, as defined in TS 36.214 [17]. Mapping of the measured quantity is defined as in TS 36.133 [18] clause 9.1.10.3. |
| ***rstd-Quality***  This field specifies the target device′s best estimate of the quality of the measured *rstd*.  When *delta-SFN* and *motionTimeSource* both included, the target device shall not include measurement errors caused by motion of the target device in *rstd-Quality* (e.g. the target device may assume the target device was stationary during OTDOA measurements). |
| ***tpIdNeighbour***  This field specifies the transmission point ID for the neighbour cell for which the RSTDs are provided. |
| ***prsIdNeighbour***  This field specifies the PRS-ID of the first PRS configuration of the neighbour cell for which the RSTDs are provided. |
| ***delta-rstd***  This field specifies the higher-resolution RSTD RSTD as defined in TS 36.133 [18] clause 9.1.10.4. Mapping of the measured quantity is defined as in TS 36.133 [18] clause 9.1.10.4. |
| ***additionalPathsNeighbour***  This field specifies one or more additional detected path timing values for the neighbour cell, relative to the path timing used for determining the *rstd* value. If this field was requested but is not included, it means the UE did not detect any additional path timing values. |
| ***nprsIdNeighbour***  This field specifies the NPRS-ID of the neighbour cell for which the RSTDs are provided. |
| ***carrierFreqOffsetNB-Neighbour***  This field specifies the offset of the NB-IoT channel number to EARFCN given by *earfcnNeighbour* as defined in TS 36.101 [21]. |
| ***delta-SFN***  This field provides information concerning the movement of the target device:  Together with *systemFrameNumber* specifies the *measurementSFN* of the RSTD reference cell when the TOA measurement for this neighbour cell has been made for determining the *rstd*. The *measurementSFN* is given by *systemFrameNumber* + *delta-SFN*. (The actual SFN is the *measurementSFN* modulo 1024.). The *measurementSFN* is used in IE *Sensor-MotionInformation* to provide movement information corresponding to the TOA measurement time.  If this field is present, the target device shall also provide the IE *Sensor-MotionInformation* in IE *Sensor‑ProvideLocationInformation*. |

#### – *OTDOA-SignalMeasurementInformation-NB*

The IE *OTDOA-SignalMeasurementInformation-NB* is used by the target device to provide RSTD measurements to the location server. The RSTD measurements are provided for a neighbour cell and the RSTD reference cell, both of which are provided in the IE *OTDOA-ProvideAssistanceData.* The RSTD reference cell may or may not be the same as the assistance data reference cell provided in *OTDOA-ReferenceCellInfo* or *OTDOA-ReferenceCellInfoNB*. If the target device stops reporting inter-frequency RSTD measurements, where the inter-frequency RSTD measurement is an OTDOA RSTD measurement with at least one cell on a frequency different from the serving cell frequency, the LPP layer shall inform lower layers that inter-frequency RSTD measurements are stopped.

NOTE 1: If there are more than 24 *NeighbourMeasurementElement-NB* to be sent, the target device may send them in multiple *ProvideLocationInformation* messages, as described under clause 5.3.

NOTE 2: If NPRS/PRS antenna ports are quasi co-located, the target device provides a single RSTD measurement for the quasi co-located antenna ports of NPRS/PRS.

-- ASN1START

OTDOA-SignalMeasurementInformation-NB-r14 ::= SEQUENCE {

systemFrameNumber-r14 BIT STRING (SIZE (10)),

physCellIdRef-r14 INTEGER (0..503),

cellGlobalIdRef-r14 ECGI OPTIONAL,

earfcnRef-r14 ARFCN-ValueEUTRA-r14 OPTIONAL, -- Cond NotSameAsRef0

referenceQuality-r14 OTDOA-MeasQuality OPTIONAL,

neighbourMeasurementList-r14 NeighbourMeasurementList-NB-r14,

tpIdRef-r14 INTEGER (0..4095) OPTIONAL, -- Cond ProvidedByServer0

prsIdRef-r14 INTEGER (0..4095) OPTIONAL, -- Cond ProvidedByServer1

additionalPathsRef-r14 AdditionalPathList-r14 OPTIONAL,

nprsIdRef-r14 INTEGER (0..4095) OPTIONAL, -- Cond ProvidedByServer2

carrierFreqOffsetNB-Ref-r14 CarrierFreqOffsetNB-r14 OPTIONAL, -- Cond NB-IoT

hyperSFN-r14 BIT STRING (SIZE (10)) OPTIONAL, -- Cond H-SFN

...

}

NeighbourMeasurementList-NB-r14 ::= SEQUENCE (SIZE(1..24)) OF NeighbourMeasurementElement-NB-r14

NeighbourMeasurementElement-NB-r14 ::= SEQUENCE {

physCellIdNeighbour-r14 INTEGER (0..503),

cellGlobalIdNeighbour-r14 ECGI OPTIONAL,

earfcnNeighbour-r14 ARFCN-ValueEUTRA-r14 OPTIONAL, -- Cond NotSameAsRef2

rstd-r14 INTEGER (0..12711),

rstd-Quality-r14 OTDOA-MeasQuality,

tpIdNeighbour-r14 INTEGER (0..4095) OPTIONAL, -- Cond ProvidedByServer0

prsIdNeighbour-r14 INTEGER (0..4095) OPTIONAL, -- Cond ProvidedByServer1

delta-rstd-r14 INTEGER (0..5) OPTIONAL,

additionalPathsNeighbour-r14

AdditionalPathList-r14 OPTIONAL,

nprsIdNeighbour-r14 INTEGER (0..4095) OPTIONAL, -- Cond ProvidedByServer2

carrierFreqOffsetNB-Neighbour-r14

CarrierFreqOffsetNB-r14 OPTIONAL, -- Cond NB-IoT

...

}

-- ASN1STOP

| Conditional presence | Explanation |
| --- | --- |
| *NotSameAsRef0* | The target device shall include this field if the EARFCN of the RSTD reference cell is not the same as the EARFCN of the assistance data reference cell provided in the OTDOA assistance data. |
| *NotSameAsRef2* | The target device shall include this field if the EARFCN of this neighbour cell is not the same as the *earfcnRef*for the RSTD reference cell. |
| *ProvidedByServer0* | The target device shall include this field if a *tpId* for this transmission point is included in the *OTDOA-ProvideAssistanceData.* Otherwise the field is absent. |
| *ProvidedByServer1* | The target device shall include this field if a *prsID* for this transmission point is included in the *OTDOA-ProvideAssistanceData.* Otherwise the field is absent. |
| *ProvidedByServer2* | The target device shall include this field if an *nprsID* for this cell is included in the *OTDOA-ProvideAssistanceData* and if this cell is a NB-IoT only cell (without associated LTE PRS cell)*.* Otherwise the field is absent. |
| *NB-IoT* | The target device shall include this field if the cell is a NB-IoT only cell (without associated LTE PRS cell). Otherwise the field is absent. |
| *H-SFN* | The target device shall include this field if it was able to determine a hyper SFN of the RSTD reference cell. |

| *OTDOA-SignalMeasurementInformation-NB* field descriptions |
| --- |
| ***systemFrameNumber***  This field specifies the SFN of the RSTD reference cell containing the starting subframe of the PRS or NPRS positioning occasion if PRS or NPRS are available on the RSTD reference cell, or subframe of the CRS for RSTD measurements if PRS and NPRS are not available on the RSTD reference cell during which the most recent neighbour cell RSTD measurement was performed.  In the case of more than a single PRS configuration on the RSTD reference cell, the first PRS configuration is referenced. |
| ***physCellIdRef***  This field specifies the physical cell identity of the RSTD reference cell. |
| ***cellGlobalIdRef***  This field specifies the ECGI, the globally unique identity of a cell in E-UTRA, of the RSTD reference cell. The target shall provide this IE if it knows the ECGI of the RSTD reference cell. |
| ***earfcnRef***  This field specifies the EARFCN of the RSTD reference cell. |
| ***referenceQuality***  This field specifies the target device′s best estimate of the quality of the TOA measurement from the RSTD reference cell, TSubframeRxRef, where TSubframeRxRef is the time of arrival of the signal from the RSTD reference cell. |
| ***neighbourMeasurementList***  This list contains the measured RSTD values for neighbour cells together with the RSTD reference cell, along with quality for each measurement. |
| ***tpIdRef***  This field specifies the transmission point ID of the RSTD reference cell. |
| ***prsIdRef***  This field specifies the PRS-ID of the first PRS configuration of the RSTD reference cell. |
| ***additionalPathsRef***  This field specifies one or more additional detected path timing values for the RSTD reference cell, relative to the path timing used for determining the *rstd* value. If this field was requested but is not included, it means the UE did not detect any additional path timing values. |
| ***nprsIdRef***  This field specifies the NPRS-ID of the RSTD reference cell. |
| ***carrierFreqOffsetNB-Ref***  This field specifies the offset of the NB-IoT channel number to EARFCN given by *earfcnRef* as defined in TS 36.101 [21]. |
| ***hyperSFN***  This field specifies the hyper SFN as defined in TS 36.331 [12] of the RSTD reference cell for the *systemFrameNumber*. |
| ***physCellIdNeighbour***  This field specifies the physical cell identity of the neighbour cell for which the RSTDs are provided. |
| ***cellGlobalIdNeighbour***  This field specifies the ECGI, the globally unique identity of a cell in E-UTRA, of the neighbour cell for which the RSTDs are provided. The target device shall provide this IE if it was able to determine the ECGI of the neighbour cell at the time of measurement. |
| ***earfcnNeighbour***  This field specifies the EARFCN of the neighbour cell used for the RSTD measurements. |
| ***rstd***  This field specifies the relative timing difference between this neighbour cell and the RSTD reference cell, as defined in TS 36.214 [17]. Mapping of the measured quantity is defined as in TS 36.133 [18] clause 9.1.10.3. |
| ***rstd-Quality***  This field specifies the target device′s best estimate of the quality of the measured *rstd*. |
| ***tpIdNeighbour***  This field specifies the transmission point ID for the neighbour cell for which the RSTDs are provided. |
| ***prsIdNeighbour***  This field specifies the PRS-ID of the first PRS configuration of the neighbour cell for which the RSTDs are provided. |
| ***delta-rstd***  This field specifies the higher-resolution RSTD RSTD as defined in TS 36.133 [18] clause 9.1.10.4. Mapping of the measured quantity is defined as in TS 36.133 [18] clause 9.1.10.4. |
| ***additionalPathsNeighbour***  This field specifies one or more additional detected path timing values for the neighbour cell, relative to the path timing used for determining the *rstd* value. If this field was requested but is not included, it means the UE did not detect any additional path timing values. |
| ***nprsIdNeighbour***  This field specifies the NPRS-ID of the neighbour cell for which the RSTDs are provided. |
| ***carrierFreqOffsetNB-Neighbour***  This field specifies the offset of the NB-IoT channel number to EARFCN given by *earfcnNeighbour* as defined in TS 36.101 [21]. |

#### – *OTDOA-MeasQuality*

-- ASN1START

OTDOA-MeasQuality ::= SEQUENCE {

error-Resolution BIT STRING (SIZE (2)),

error-Value BIT STRING (SIZE (5)),

error-NumSamples BIT STRING (SIZE (3)) OPTIONAL,

...

}

-- ASN1STOP

| *OTDOA-MeasQuality* field descriptions |
| --- |
| ***error-Resolution***  This field specifies the resolution R used in *error-Value* field. The encoding on two bits is as follows:  ′00′ 5 metres  ′01′ 10 metres  ′10′ 20 metres  ′11′ 30 metres |
| ***error-Value***  This field specifies the target device′s best estimate of the uncertainty of the OTDOA (or TOA) measurement.  The encoding on five bits is as follows:  ′00000′ 0 to (R\*1-1) metres  ′00001′ R\*1 to (R\*2-1) metres  ′00010′ R\*2 to (R\*3-1) metres  …  ′11111′ R\*31 metres or more;  where R is the resolution defined by *error-Resolution*field.  E.g., R=20 m corresponds to 0-19 m, 20-39 m,…,620+ m. |
| ***error-NumSamples***  If the *error-Value*field provides the sample uncertainty of the OTDOA (or TOA) measurement, this field specifies how many measurements have been used by the target device to determine this (i.e., sample size). Following 3 bit encoding is used:  ′000′ Not the baseline metric  ′001′ 5-9  ′010′ 10-14  ′011′ 15-24  ′100′ 25-34  ′101′ 35-44  ′110′ 45-54  ′111′ 55 or more.  In the case of the value ′000′, the *error-Value* field contains the target device′s best estimate of the uncertainty of the OTDOA (or TOA) measurement not based on the baseline metric. E.g., other measurements such as signal-to-noise-ratio or signal strength can be utilized to estimate the *error-Value.*  If this field is absent, the value of this field is ′000′. |

#### – *AdditionalPath*

The IE *AdditionalPath* is used by the target device to provide information about additional paths associated with the RSTD measurements in the form of a relative time difference and a quality value. The additional path *relativeTimeDifference* is the detected path timing relative to the detected path timing used for the *rstd* value (TS 36.214 [17]), and each additional path can be associated with a quality value *path-Quality.*

-- ASN1START

AdditionalPath-r14 ::= SEQUENCE {

relativeTimeDifference-r14 INTEGER (-256..255),

path-Quality-r14 OTDOA-MeasQuality OPTIONAL,

...

}

-- ASN1STOP

| *AdditionalPath* field descriptions |
| --- |
| ***relativeTimeDifference***  This field specifies the additional detected path timing relative to the detected path timing used for the *rstd* value in units of 0.5 Ts, with Ts=1/(15000\*2048) seconds. A positive value indicates that the particular path is later in time than the detected path used for RSTD; a negative value indicates that the particular path is earlier in time than the detected path used for RSTD. |
| ***path-Quality***  This field specifies the target device′s best estimate of the quality of the detected timing of the additional path. |

#### 6.5.1.6 OTDOA Location Information Request

#### – *OTDOA-RequestLocationInformation*

The IE *OTDOA-RequestLocationInformation* is used by the location server to request OTDOA location measurements from a target device. Details of the required measurements (e.g. details of assistance data reference cell and neighbour cells) are conveyed in the *OTDOA-ProvideAssistanceData* IE in a separate Provide Assistance Data message.

-- ASN1START

OTDOA-RequestLocationInformation ::= SEQUENCE {

assistanceAvailability BOOLEAN,

...,

[[

multipathRSTD-r14 ENUMERATED { requested } OPTIONAL, -- Need ON

maxNoOfRSTDmeas-r14 INTEGER (1..32) OPTIONAL -- Need ON

]],

[[

motionMeasurements-r15 ENUMERATED { requested } OPTIONAL -- Need ON

]]

}

-- ASN1STOP

| *OTDOA-RequestLocationInformation* field descriptions |
| --- |
| ***assistanceAvailability***  This field indicates whether the target device may request additional OTDOA assistance data from the server. TRUE means allowed and FALSE means not allowed. |
| ***multipathRSTD***  This field, if present, indicates that the target device is requested to report additional detected path timing information per RSTD reference and neighbour cell. |
| ***maxNoOfRSTDmeas***  This field, if present, indicates the maximum number of *NeighbourMeasurementElement* fields (i.e., RSTD measurements) the target device can provide in *OTDOA-SignalMeasurementInformation*. |
| ***motionMeasurements***  This field, if present, indicates that the target device is requested to report the motion measurements (*delta-SFN* and *motionTimeSource*) in *OTDOA‑SignalMeasurementInformation* as well as the IE *Sensor-MotionInformation* in IE *Sensor‑ProvideLocationInformation*. |

#### 6.5.1.7 OTDOA Capability Information

#### – *OTDOA-ProvideCapabilities*

The IE *OTDOA-ProvideCapabilities* is used by the target device to indicate its capability to support OTDOA and to provide its OTDOA positioning capabilities to the location server.

-- ASN1START

OTDOA-ProvideCapabilities ::= SEQUENCE {

otdoa-Mode BIT STRING { ue-assisted (0),

ue-assisted-NB-r14 (1),

ue-assisted-NB-TDD-r15 (2) } (SIZE (1..8)),

...,

supportedBandListEUTRA SEQUENCE (SIZE (1..maxBands)) OF SupportedBandEUTRA OPTIONAL,

supportedBandListEUTRA-v9a0 SEQUENCE (SIZE (1..maxBands)) OF SupportedBandEUTRA-v9a0

OPTIONAL,

interFreqRSTDmeasurement-r10 ENUMERATED { supported } OPTIONAL,

additionalNeighbourCellInfoList-r10 ENUMERATED { supported } OPTIONAL,

prs-id-r14 ENUMERATED { supported } OPTIONAL,

tp-separation-via-muting-r14 ENUMERATED { supported } OPTIONAL,

additional-prs-config-r14 ENUMERATED { supported } OPTIONAL,

prs-based-tbs-r14 ENUMERATED { supported } OPTIONAL,

additionalPathsReport-r14 ENUMERATED { supported } OPTIONAL,

densePrsConfig-r14 ENUMERATED { supported } OPTIONAL,

maxSupportedPrsBandwidth-r14 ENUMERATED { n6, n15, n25, n50, n75, n100, ...} OPTIONAL,

prsOccGroup-r14 ENUMERATED { supported } OPTIONAL,

prsFrequencyHopping-r14 ENUMERATED { supported } OPTIONAL,

maxSupportedPrsConfigs-r14 ENUMERATED { c2, c3 } OPTIONAL,

periodicalReporting-r14 ENUMERATED { supported } OPTIONAL,

multiPrbNprs-r14 ENUMERATED { supported } OPTIONAL,

idleStateForMeasurements-r14 ENUMERATED { required } OPTIONAL,

numberOfRXantennas-r14 ENUMERATED { rx1, ... } OPTIONAL,

motionMeasurements-r15 ENUMERATED { supported } OPTIONAL,

interRAT-RSTDmeasurement-r15 ENUMERATED { supported } OPTIONAL,

scheduledLocationRequestSupported-r17 ScheduledLocationTimeSupport-r17 OPTIONAL,

periodicReportingIntervalMsSupport-r18 PeriodicReportingIntervalMsSupport-r18 OPTIONAL

}

maxBands INTEGER ::= 64

SupportedBandEUTRA ::= SEQUENCE {

bandEUTRA INTEGER (1..maxFBI)

}

SupportedBandEUTRA-v9a0 ::= SEQUENCE {

bandEUTRA-v9a0 INTEGER (maxFBI-Plus1..maxFBI2) OPTIONAL

}

maxFBI INTEGER ::= 64 -- Maximum value of frequency band indicator

maxFBI-Plus1 INTEGER ::= 65 -- lowest value extended FBI range

maxFBI2 INTEGER ::= 256 -- highest value extended FBI range

-- ASN1STOP

| *OTDOA-ProvideCapabilities* field descriptions |
| --- |
| ***otdoa-Mode***  This field specifies the OTDOA mode(s) supported by the target device. This is represented by a bit string, with a one value at the bit position means the particular OTDOA mode is supported; a zero value means not supported. A zero-value in all bit positions in the bit string means OTDOA positioning method is not supported by the target device.  ue-assisted: Bit 0 indicates that the target device supports UE-assisted OTDOA and LTE PRS.  ue-assisted-NB: Bit 1 indicates that the target device supports UE-assisted OTDOA and NB-IoT NPRS.  ue-assisted-NB-TDD: Bit 2 indicates that the target device supports UE-assisted OTDOA and NB-IoT NPRS for TDD. |
| ***SupportedBandEUTRA***  This field specifies the frequency bands for which the target device supports RSTD measurements. One entry corresponding to each supported E-UTRA band as defined in TS 36.101 [21]. In the case the target device includes *bandEUTRA-v9a0*, the target device shall set the corresponding entry of *bandEUTRA* (i.e. without suffix) to *maxFBI*. |
| ***interFreqRSTDmeasurement***  This field, if present, indicates that the target device supports inter-frequency RSTD measurements within and between the frequency bands indicated in *SupportedBandEUTRA*. |
| ***additionalNeighbourCellInfoList***  This field, if present, indicates that the target device supports up to 3×24 *OTDOA-NeighbourCellInfoElement* in *OTDOA‑NeighbourCellInfoList* in *OTDOA-ProvideAssistanceData* without any restriction for the *earfcn* in each *OTDOA-NeighbourCellInfoElement* as specified in clause 6.5.1.2. |
| ***prs-id***  This field, if present, indicates that the target device supports PRS generation based on the PRS-ID as specified in TS 36.211 [16] and support for TP-ID in *OTDOA-ReferenceCellInfo* and *OTDOA-NeighbourCellInfoList*. |
| ***tp-separation-via-muting***  This field, if present, indicates that the target device supports RSTD measurements for cells which have associated transmission points (e.g., Remote Radio Heads) within the cell coverage and where these associated transmission points have the same physical cell identity as the associated cell, and where these transmission points are identified via a different muting pattern. The field also indicates support for TP-ID in *OTDOA-ReferenceCellInfo* and *OTDOA‑NeighbourCellInfoList*. |
| ***additional-prs-config***  This field, if present, indicates that the target device supports additional PRS configurations. The additional PRS configuration in *PRS-Info* IE comprise:  - support for *prs-ConfigurationIndex* > 2399; - support for NPRS values in addition to 1, 2, 4 and 6 (*add-numDL-Frames in PRS-Info);*  - support for muting bit string lengths > 16 bits. |
| ***prs-based-tbs***  This field, if present, indicates that the target device supports RSTD measurements for PRS-only TPs. |
| ***additionalPathsReport***  This field, if present, indicates that the target device supports reporting of timing information for additional detected paths for RSTD reference and each neighbour cell. |
| ***densePrsConfig***  This field, if present, indicates that the target device supports a subset of the additional PRS configurations associated with capability *additional-prs-config* which comprises:  - support for *prs-ConfigurationIndex* > 2404;  - support for NPRS values of 10, 20, 40, 80 and 160 (in addition to 1, 2, 4 and 6).  In the case *additional-prs-config* is present, this field is not present. |
| ***maxSupportedPrsBandwidth***  This field, if present, indicates the maximum PRS bandwidth supported by the target device. Enumerated value n6 corresponds to 6 resource blocks, n15 to 15 resource blocks and so on. If this field is not present, the target device is assumed to support the PRS bandwidth associated with the target device type, which for LTE devices including Cat-M1/M2 is 100 resource blocks and for NB-IoT devices is 1 resource block. |
| ***prsOccGroup***  This field, if present, indicates that the target device supports PRS occasion groups, which implies that each bit of a configured muting pattern applies per PRS occasion group. |
| ***prsFrequencyHopping***  This field, if present, indicates that the target device supports PRS occasion frequency hopping, as specified in TS 36.211 [16]. |
| ***maxSupportedPrsConfigs***  This field, if present, indicates that the target device supports multiple PRS configurations per cell. Enumerated value c2 indicates support for up to 2 configurations; c3 indicates support for up to 3 configurations. |
| ***periodicalReporting***  This field, if present, indicates that the target device supports *periodicalReporting* of RSTD measurements*.* If this field is absent, the location server may assume that the target device does not support *periodicalReporting* in *CommonIEsRequestLocationInformation*. |
| ***multiPrbNprs***  This field, if present, indicates that the target device supports NPRS configuration in more than one resource block (i.e., *maxCarrier* in *PRS-Info-NB* greater than 1). |
| ***idleStateForMeasurements***  This field, if present, indicates that the target device requires idle state to perform RSTD measurements. |
| ***numberOfRXantennas***  This field is not applicable to NB-IoT devices.  This field, if present, indicates the number of UE downlink receive antennas for RSTD measurements (see TS 36.133 [18]). Enumerated value rx1 indicates a single antenna receiver. If this field is absent, the target device is assumed to support two RX antennas for RSTD measurements. |
| ***motionMeasurements***  This field, if present, indicates that the target device supports reporting of motion measurements (*delta-SFN* and *motionTimeSource*) in *OTDOA‑SignalMeasurementInformation*. The presence of this field implies presence of *sensor-MotionInformationSup* in IE *Sensor‑ProvideCapabilities*. |
| ***interRAT-RSTDmeasurement***  This field, if present, indicates that the target device supports inter-RAT RSTD measurements (TS 38.215 [36]); i.e., E-UTRA RSTD measurements when the target device is served by an NR cell. |
| ***scheduledLocationRequestSupported***  This field, if present, indicates that the target device supports scheduled location requests – i.e., supports the IE *ScheduledLocationTime* in IE *CommonIEsRequestLocationInformation* – and the time base(s) supported for the scheduled location time. |
| ***periodicReportingIntervalMsSupport***  This field, if present, indicates that the target device supports millisecond periodic reporting intervals for location information – i.e., supports the subfield *reportingIntervalMs* of the IE *PeriodicalReportingCriteriaExt* in IE *CommonIEsRequestLocationInformation* – and the minimum millisecond report interval supported for the periodic reporting. |

#### 6.5.1.8 OTDOA Capability Information Request

#### – *OTDOA-RequestCapabilities*

The IE *OTDOA-RequestCapabilities* is used by the location server to request the capability of the target device to support OTDOA and to request OTDOA positioning capabilities from a target device.

-- ASN1START

OTDOA-RequestCapabilities ::= SEQUENCE {

...

}

-- ASN1STOP

#### 6.5.1.9 OTDOA Error Elements

#### – *OTDOA-Error*

The IE *OTDOA-Error* is used by the location server or target device to provide OTDOA error reasons to the target device or location server, respectively.

-- ASN1START

OTDOA-Error ::= CHOICE {

locationServerErrorCauses OTDOA-LocationServerErrorCauses,

targetDeviceErrorCauses OTDOA-TargetDeviceErrorCauses,

...

}

-- ASN1STOP

#### – *OTDOA-LocationServerErrorCauses*

The IE *OTDOA-LocationServerErrorCauses* is used by the location server to provide OTDOA error reasons to the target device.

-- ASN1START

OTDOA-LocationServerErrorCauses ::= SEQUENCE {

cause ENUMERATED { undefined,

assistanceDataNotSupportedByServer,

assistanceDataSupportedButCurrentlyNotAvailableByServer,

...

},

...

}

-- ASN1STOP

#### – *OTDOA-TargetDeviceErrorCauses*

The IE *OTDOA-TargetDeviceErrorCauses* is used by the target device to provide OTDOA error reasons to the location server.

-- ASN1START

OTDOA-TargetDeviceErrorCauses ::= SEQUENCE {

cause ENUMERATED { undefined,

assistance-data-missing,

unableToMeasureReferenceCell,

unableToMeasureAnyNeighbourCell,

attemptedButUnableToMeasureSomeNeighbourCells,

...

},

...

}

-- ASN1STOP

### 6.5.2 A-GNSS Positioning

#### 6.5.2.1 GNSS Assistance Data

#### – *A-GNSS-ProvideAssistanceData*

The IE *A-GNSS-ProvideAssistanceData* is used by the location server to provide assistance data to enable UE‑based and UE‑assisted A‑GNSS. It may also be used to provide GNSS positioning specific error reasons.

-- ASN1START

A-GNSS-ProvideAssistanceData ::= SEQUENCE {

gnss-CommonAssistData GNSS-CommonAssistData OPTIONAL, -- Need ON

gnss-GenericAssistData GNSS-GenericAssistData OPTIONAL, -- Need ON

gnss-Error A-GNSS-Error OPTIONAL, -- Need ON

...,

[[

gnss-PeriodicAssistData-r15 GNSS-PeriodicAssistData-r15 OPTIONAL -- Cond CtrTrans

]]

}

-- ASN1STOP

| Conditional presence | Explanation |
| --- | --- |
| *CtrTrans* | The field is mandatory present in the control transaction of a periodic assistance data delivery session as described in clauses 5.2.1a and 5.2.2a. Otherwise it is not present. |

#### – *GNSS-CommonAssistData*

The IE *GNSS-CommonAssistData* is used by the location server to provide assistance data which can be used for any GNSS.

-- ASN1START

GNSS-CommonAssistData ::= SEQUENCE {

gnss-ReferenceTime GNSS-ReferenceTime OPTIONAL, -- Need ON

gnss-ReferenceLocation GNSS-ReferenceLocation OPTIONAL, -- Need ON

gnss-IonosphericModel GNSS-IonosphericModel OPTIONAL, -- Need ON

gnss-EarthOrientationParameters GNSS-EarthOrientationParameters OPTIONAL, -- Need ON

...,

[[

gnss-RTK-ReferenceStationInfo-r15

GNSS-RTK-ReferenceStationInfo-r15 OPTIONAL, -- Need ON

gnss-RTK-CommonObservationInfo-r15

GNSS-RTK-CommonObservationInfo-r15 OPTIONAL, -- Cond RTK

gnss-RTK-AuxiliaryStationData-r15

GNSS-RTK-AuxiliaryStationData-r15 OPTIONAL -- Need ON

]],

[[

gnss-SSR-CorrectionPoints-r16

GNSS-SSR-CorrectionPoints-r16 OPTIONAL -- Need ON

]],

[[

gnss-Integrity-ServiceParameters-r17

GNSS-Integrity-ServiceParameters-r17 OPTIONAL, -- Need ON

gnss-Integrity-ServiceAlert-r17

GNSS-Integrity-ServiceAlert-r17 OPTIONAL -- Need OR

]],

[[

gnss-los-nlos-GridPoints-r18 GNSS-LOS-NLOS-GridPoints-r18 OPTIONAL, -- Need ON

gnss-SSR-IOD-Update-r18 GNSS-SSR-IOD-Update-r18 OPTIONAL -- Need OR

]]

}

-- ASN1STOP

| Conditional presence | Explanation |
| --- | --- |
| *RTK* | The field is mandatory present if the IE *GNSS-RTK-Observations* is included in IE *GNSS‑GenericAssistData*; otherwise it is not present. |

#### – *GNSS-GenericAssistData*

The IE *GNSS-GenericAssistData* is used by the location server to provide assistance data for a specific GNSS. The specific GNSS for which the provided assistance data are applicable is indicated by the IE *GNSS‑ID* and (if applicable) by the IE *SBAS‑ID*. Assistance for up to 16 GNSSs can be provided.

-- ASN1START

GNSS-GenericAssistData ::= SEQUENCE (SIZE (1..16)) OF GNSS-GenericAssistDataElement

GNSS-GenericAssistDataElement ::= SEQUENCE {

gnss-ID GNSS-ID,

sbas-ID SBAS-ID OPTIONAL, -- Cond GNSS-ID-SBAS

gnss-TimeModels GNSS-TimeModelList OPTIONAL, -- Need ON

gnss-DifferentialCorrections GNSS-DifferentialCorrections OPTIONAL, -- Need ON

gnss-NavigationModel GNSS-NavigationModel OPTIONAL, -- Need ON

gnss-RealTimeIntegrity GNSS-RealTimeIntegrity OPTIONAL, -- Need ON

gnss-DataBitAssistance GNSS-DataBitAssistance OPTIONAL, -- Need ON

gnss-AcquisitionAssistance GNSS-AcquisitionAssistance OPTIONAL, -- Need ON

gnss-Almanac GNSS-Almanac OPTIONAL, -- Need ON

gnss-UTC-Model GNSS-UTC-Model OPTIONAL, -- Need ON

gnss-AuxiliaryInformation GNSS-AuxiliaryInformation OPTIONAL, -- Need ON

...,

[[

bds-DifferentialCorrections-r12

BDS-DifferentialCorrections-r12 OPTIONAL, -- Cond GNSS-ID-BDS

bds-GridModel-r12 BDS-GridModelParameter-r12 OPTIONAL -- Cond GNSS-ID-BDS

]],

[[

gnss-RTK-Observations-r15 GNSS-RTK-Observations-r15 OPTIONAL, -- Need ON

glo-RTK-BiasInformation-r15 GLO-RTK-BiasInformation-r15 OPTIONAL, -- Cond GNSS-ID-GLO

gnss-RTK-MAC-CorrectionDifferences-r15

GNSS-RTK-MAC-CorrectionDifferences-r15

OPTIONAL, -- Need ON

gnss-RTK-Residuals-r15 GNSS-RTK-Residuals-r15 OPTIONAL, -- Need ON

gnss-RTK-FKP-Gradients-r15 GNSS-RTK-FKP-Gradients-r15 OPTIONAL, -- Need ON

gnss-SSR-OrbitCorrections-r15

GNSS-SSR-OrbitCorrections-r15 OPTIONAL, -- Need ON

gnss-SSR-ClockCorrections-r15

GNSS-SSR-ClockCorrections-r15 OPTIONAL, -- Need ON

gnss-SSR-CodeBias-r15 GNSS-SSR-CodeBias-r15 OPTIONAL -- Need ON

]],

[[

gnss-SSR-URA-r16 GNSS-SSR-URA-r16 OPTIONAL, -- Need ON

gnss-SSR-PhaseBias-r16 GNSS-SSR-PhaseBias-r16 OPTIONAL, -- Need ON

gnss-SSR-STEC-Correction-r16 GNSS-SSR-STEC-Correction-r16

OPTIONAL, -- Need ON

gnss-SSR-GriddedCorrection-r16 GNSS-SSR-GriddedCorrection-r16

OPTIONAL, -- Need ON

navic-DifferentialCorrections-r16 NavIC-DifferentialCorrections-r16

OPTIONAL, -- Cond GNSS-ID-NavIC

navic-GridModel-r16 NavIC-GridModelParameter-r16

OPTIONAL -- Cond GNSS-ID-NavIC

]],

[[

gnss-SSR-OrbitCorrectionsSet2-r17 GNSS-SSR-OrbitCorrectionsSet2-r17

OPTIONAL, -- Need ON

gnss-SSR-ClockCorrectionsSet2-r17 GNSS-SSR-ClockCorrectionsSet2-r17

OPTIONAL, -- Need ON

gnss-SSR-URA-Set2-r17 GNSS-SSR-URA-Set2-r17 OPTIONAL -- Need ON

]],

[[

gnss-LOS-NLOS-GriddedIndications-r18 GNSS-LOS-NLOS-GriddedIndications-r18

OPTIONAL, -- Need ON

gnss-SSR-SatellitePCVResiduals-r18 GNSS-SSR-SatellitePCVResiduals-r18

OPTIONAL -- Need ON

]]

}

-- ASN1STOP

| Conditional presence | Explanation |
| --- | --- |
| *GNSS‑ID‑SBAS* | The field is mandatory present if the *GNSS‑ID* = *sbas*; otherwise it is not present. |
| *GNSS‑ID‑BDS* | The field may be present if the *GNSS‑ID* = *bds*; otherwise it is not present. |
| *GNSS-ID-GLO* | The field is optionally present, need ON, if the *GNSS ID* = *glonass*; otherwise it is not present. |
| *GNSS-ID-NAVIC* | The field is optionally present, need ON, if the *GNSS‑ID* = *navic*; otherwise it is not present |

#### *– GNSS-PeriodicAssistData*

The IE *GNSS-PeriodicAssistData* is used by the location server to provide control parameters for a periodic assistance data delivery session (e.g., interval and duration) to the target device.

NOTE: Omission of a particular assistance data type field in IE *GNSS-PeriodicAssistData* means that the location server does not provide this assistance data type in a data transaction of a periodic assistance data delivery session, as described in clauses 5.2.1a and 5.2.2a. Inclusion of no assistance data type fields in IE *GNSS-PeriodicAssistData* means that a periodic assistance data delivery session is terminated.

-- ASN1START

GNSS-PeriodicAssistData-r15 ::= SEQUENCE {

gnss-RTK-PeriodicObservations-r15 GNSS-PeriodicControlParam-r15 OPTIONAL, -- Need ON

glo-RTK-PeriodicBiasInformation-r15 GNSS-PeriodicControlParam-r15 OPTIONAL, -- Need ON

gnss-RTK-MAC-PeriodicCorrectionDifferences-r15

GNSS-PeriodicControlParam-r15 OPTIONAL, -- Need ON

gnss-RTK-PeriodicResiduals-r15 GNSS-PeriodicControlParam-r15 OPTIONAL, -- Need ON

gnss-RTK-FKP-PeriodicGradients-r15 GNSS-PeriodicControlParam-r15 OPTIONAL, -- Need ON

gnss-SSR-PeriodicOrbitCorrections-r15

GNSS-PeriodicControlParam-r15 OPTIONAL, -- Need ON

gnss-SSR-PeriodicClockCorrections-r15

GNSS-PeriodicControlParam-r15 OPTIONAL, -- Need ON

gnss-SSR-PeriodicCodeBias-r15 GNSS-PeriodicControlParam-r15 OPTIONAL, -- Need ON

...,

[[

gnss-SSR-PeriodicURA-r16 GNSS-PeriodicControlParam-r15 OPTIONAL, -- Need ON

gnss-SSR-PeriodicPhaseBias-r16 GNSS-PeriodicControlParam-r15 OPTIONAL, -- Need ON

gnss-SSR-PeriodicSTEC-Correction-r16 GNSS-PeriodicControlParam-r15 OPTIONAL, -- Need ON

gnss-SSR-PeriodicGriddedCorrection-r16 GNSS-PeriodicControlParam-r15 OPTIONAL -- Need ON

]],

[[

gnss-Integrity-PeriodicServiceAlert-r17 GNSS-PeriodicControlParam-r15 OPTIONAL -- Need ON

]],

[[

gnss-SSR-PeriodicOrbitCorrectionsSet2-r17

GNSS-PeriodicControlParam-r15 OPTIONAL, -- Need ON

gnss-SSR-PeriodicClockCorrectionsSet2-r17

GNSS-PeriodicControlParam-r15 OPTIONAL, -- Need ON

gnss-SSR-PeriodicURA-Set2-r17 GNSS-PeriodicControlParam-r15 OPTIONAL -- Need ON

]],

[[

gnss-SSR-PeriodicIOD-Update-r18 GNSS-PeriodicControlParam-r15 OPTIONAL -- Need OR

]]

}

-- ASN1STOP

#### 6.5.2.2 GNSS Assistance Data Elements

#### – *GNSS-ReferenceTime*

The IE *GNSS-ReferenceTime* is used by the location server to provide the GNSS specific system time with uncertainty and the relationship between GNSS system time and network air-interface timing of the eNodeB/NodeB/BTS transmission in the reference cell.

If the IE *networkTime* is present, the IEs *gnss-SystemTime* and *networkTime* provide a valid relationship between GNSS system time and air-interface network time, as seen at the approximate location of the target device, i.e. the propagation delay from the gNB/ng-eNB/eNodeB/NodeB/BTS to the target device is compensated for by the location server. Depending on implementation, the relation between GNSS system time and air-interface network time may have varying accuracy. The uncertainty of this timing relation is provided in the IE *referenceTimeUnc*. If the propagation delay from the eNodeB/NodeB/BTS to the target device is not accurately known, the location server uses the best available approximation of the propagation delay and take the corresponding delay uncertainty into account in the calculation of the IE *referenceTimeUnc*.

If the IE *networkTime* is not present, the IE *gnssSystemTime* is an estimate of current GNSS system time at time of reception of the IE *GNSS-ReferenceTime* by the target device. The location server should achieve an accuracy of +/- 3 seconds for this estimate including allowing for the transmission delay between the location server and the target device. Note that the target device should further compensate *gnss-SystemTime* for the time between the reception of *GNSS-ReferenceTime* and the time when the *gnss-SystemTime* is used.

The location server provides a value for the *gnss-TimeID* only for GNSSs supported by the target device.

The IE *GNSS-ReferenceTimeForOneCell* can be provided multiple times (up to 16) to provide fine time assistance for several (neighbour) cells.

-- ASN1START

GNSS-ReferenceTime ::= SEQUENCE {

gnss-SystemTime GNSS-SystemTime,

referenceTimeUnc INTEGER (0..127) OPTIONAL, -- Cond noFTA

gnss-ReferenceTimeForCells SEQUENCE (SIZE (1..16)) OF

GNSS-ReferenceTimeForOneCell OPTIONAL, -- Need ON

...

}

GNSS-ReferenceTimeForOneCell ::= SEQUENCE {

networkTime NetworkTime,

referenceTimeUnc INTEGER (0..127),

bsAlign ENUMERATED {true} OPTIONAL,

...

}

-- ASN1STOP

| Conditional presence | Explanation |
| --- | --- |
| *noFTA* | The field may be present if *gnss-ReferenceTimeForCells* is absent; otherwise it is not present. |

| *GNSS-ReferenceTime* field descriptions |
| --- |
| ***gnss-SystemTime***  This field provides the specific GNSS system time. |
| ***networkTime***  This field specifies the cellular network time at the epoch corresponding to *gnss-SystemTime.* |
| ***referenceTimeUnc***  This field provides the accuracy of the relation between *gnssSystemTime* and *networkTime* time if IE *networkTime* is provided. When IE *networkTime* is not provided, this field can be included to provide the accuracy of the provided *gnssSystemTime*.  If GNSS TOD is the given GNSS time, then the true GNSS time, corresponding to the provided network time as observed at the target device location, lies in the interval [GNSS TOD - *referenceTimeUnc*, GNSS TOD + *referenceTimeUnc*].  The uncertainty *r*, expressed in microseconds, is mapped to a number *K*, with the following formula:  *r* = C\*(((1+x)K)-1)  with C = 0.5 and x = 0.14. To encode any higher value of uncertainty than that corresponding in the above formula to K=127, the same value, K=127, shall also be used. The uncertainty is then coded on 7 bits, as the binary encoding of K. Example values for the *referenceTimeUnc* Format: see table K to uncertainty relation below. |
| ***bsAlign***  This flag, if present, indicates that the transmission timings of all cells sharing, depending on the RAT, the same carrier frequency and Tracking Area/Location Area/Routing Area as the cell indicated, are frame aligned. This information allows the target device to derive the GNSS - cellular time relation for any of these cells based on the timing relation information provided in *GNSS-ReferenceTime*. The flag should be set consistently in all these cells. This flag does not guarantee SFN alignment. |

K to uncertainty relation

|  |  |
| --- | --- |
| Value of K | Value of uncertainty |
| 0 | 0 nanoseconds |
| 1 | 70 nanoseconds |
| 2 | 149.8 nanoseconds |
| - | - |
| 50 | 349.62 microseconds |
| - | - |
| 127 | ≥ 8.43 seconds |

#### – *GNSS-SystemTime*

-- ASN1START

GNSS-SystemTime ::= SEQUENCE {

gnss-TimeID GNSS-ID,

gnss-DayNumber INTEGER (0..32767),

gnss-TimeOfDay INTEGER (0..86399),

gnss-TimeOfDayFrac-msec INTEGER (0..999) OPTIONAL, -- Need ON

notificationOfLeapSecond BIT STRING (SIZE(2)) OPTIONAL, -- Cond gnss-TimeID-glonass

gps-TOW-Assist GPS-TOW-Assist OPTIONAL, -- Cond gnss-TimeID-gps

...

}

-- ASN1STOP

| Conditional presence | Explanation |
| --- | --- |
| *gnss-TimeID-glonass* | The field may be present if *gnss-TimeID*=`glonass′; otherwise it is not present. |
| *gnss-TimeID-gps* | The field may be present if *gnss-TimeID*=`gps′; otherwise it is not present. |

| *GNSS-SystemTime* field descriptions |
| --- |
| ***gnss-TimeID***  This field specifies the GNSS for which the *GNSS-SystemTime* is provided. |
| ***gnss-DayNumber***  This field specifies the sequential number of days (with day count starting at 0) from the origin of the GNSS System Time as follows:  GPS, QZSS, SBAS – Days from January 6th 1980 00:00:00 UTC (USNO);  Galileo – Days from Galileo System Time (GST) start epoch, defined as 13 seconds before midnight between 21st August and 22nd August 1999; i.e., GST was equal to 13 seconds at August 22nd 1999 00:00:00 UTC;  GLONASS – Days from December 31st 1995 21:00:00 UTC (SU), which is local UTC Moscow  January 1st 1996 00:00:00, defined as UTC(SU) + 3 hours in [9];  BDS – Days from January 1st 2006 00:00:00 UTC (NTSC).  NavIC – Days from NavIC System Time start epoch, defined as 13 seconds before midnight between 21st  August and 22nd August 1999; i.e., NavIC System Time was equal to 00:00:00 at August 21st, 1999  23:59:47 UTC (BIPM). |
| ***gnss-TimeOfDay***  This field specifies the integer number of seconds from the GNSS day change. |
| ***gnss-TimeOfDayFrac-msec***  This field specifies the fractional part of the *gnssTimeOfDay* field in 1‑milli‑seconds resolution. The total GNSS TOD is *gnss-TimeOfDay + gnssTimeOfDayFrac-msec.* |
| ***notificationOfLeapSecond***  This field specifies the notification of forthcoming leap second correction, as defined by parameter KP in [9, Table 4.7]. |
| ***gps-TOW-Assist***  This field contains several fields in the Telemetry (TLM) Word and Handover Word (HOW) that are currently being broadcast by the respective GPS satellites. Combining this information with GPS TOW enables the target device to know the entire 1.2-second (60-bit) pattern of TLM and HOW that is transmitted at the start of each six-second NAV subframe by the particular GPS satellite. |

#### – *GPS-TOW-Assist*

-- ASN1START

GPS-TOW-Assist ::= SEQUENCE (SIZE(1..64)) OF GPS-TOW-AssistElement

GPS-TOW-AssistElement ::= SEQUENCE {

satelliteID INTEGER (1..64),

tlmWord INTEGER (0..16383),

antiSpoof INTEGER (0..1),

alert INTEGER (0..1),

tlmRsvdBits INTEGER (0..3),

...

}

-- ASN1STOP

| *GPS-TOW-Assist* field descriptions |
| --- |
| ***satelliteID***  This field identifies the satellite for which the *GPS-TOW-Assist* is applicable. This field is identical to the GPS PRN Signal No. defined in [4]. |
| ***tlmWord***  This field contains a 14-bit value representing the Telemetry Message (TLM) being broadcast by the GPS satellite identified by the particular *satelliteID*, with the MSB occurring first in the satellite transmission, as defined in [4]. |
| ***antiSpoof***  This field contains the Anti-Spoof flag that is being broadcast by the GPS satellite identified by *satelliteID*, as defined in [4]. |
| ***alert***  This field contains the Alert flag that is being broadcast by the GPS satellite identified by *satelliteID*, as defined in [4]. |
| ***tlmRsvdBits***  This field contains the two reserved bits in the TLM Word being broadcast by the GPS satellite identified by *satelliteID*, with the MSB occurring first in the satellite transmission, as defined in [4]. |

#### – *NetworkTime*

-- ASN1START

NetworkTime ::= SEQUENCE {

secondsFromFrameStructureStart INTEGER(0..12533),

fractionalSecondsFromFrameStructureStart INTEGER(0..3999999),

frameDrift INTEGER (-64..63) OPTIONAL, -- Cond GNSSsynch

cellID CHOICE {

eUTRA SEQUENCE {

physCellId INTEGER (0..503),

cellGlobalIdEUTRA CellGlobalIdEUTRA-AndUTRA OPTIONAL, -- Need ON

earfcn ARFCN-ValueEUTRA,

...,

[[ earfcn-v9a0 ARFCN-ValueEUTRA-v9a0 OPTIONAL -- Cond EARFCN-max

]]

},

uTRA SEQUENCE {

mode CHOICE {

fdd SEQUENCE {

primary-CPICH-Info INTEGER (0..511),

...

},

tdd SEQUENCE {

cellParameters INTEGER (0..127),

...

}

},

cellGlobalIdUTRA CellGlobalIdEUTRA-AndUTRA OPTIONAL, -- Need ON

uarfcn ARFCN-ValueUTRA,

...

},

gSM SEQUENCE {

bcchCarrier INTEGER (0..1023),

bsic INTEGER (0..63),

cellGlobalIdGERAN CellGlobalIdGERAN OPTIONAL, -- Need ON

...

},

...,

nBIoT-r14 SEQUENCE {

nbPhysCellId-r14 INTEGER (0..503),

nbCellGlobalId-r14 ECGI OPTIONAL, -- Need ON

nbCarrierFreq-r14 CarrierFreq-NB-r14,

...

},

nr-r15 SEQUENCE {

nrPhysCellId-r15 INTEGER (0..1007),

nrCellGlobalID-r15 NCGI-r15 OPTIONAL, -- Need ON

nrARFCN-r15 ARFCN-ValueNR-r15,

...

}

},

...

}

-- ASN1STOP

|  |  |
| --- | --- |
| Conditional presence | Explanation |
| *EARFCN-max* | The field is mandatory present if the corresponding *earfcn* (i.e. without suffix) is set to *maxEARFCN*. Otherwise the field is not present. |
| *GNSSsynch* | The field is present and set to 0 if *NetworkTime* is synchronized to *gnss-SystemTime*; otherwise the field is optionally present, need OR. |

| *NetworkTime* field descriptions |
| --- |
| ***secondsFromFrameStructureStart***  This field specifies the number of seconds from the beginning of the longest frame structure in the corresponding air interface.  In the case of E-UTRA, the SFN cycle length is 10.24 seconds.  In the case of UTRA, the SFN cycle length is 40.96 seconds.  In the case of GSM, the hyperfame length is 12533.76 seconds.  In the case of NB-IoT, the Hyper-SFN cycle lengths is 10485.76 seconds.  In the case of NR, the SFN cycle length is 10.24 seconds. |
| ***fractionalSecondsFromFrameStructureStart***  This field specifies the fractional part of the *secondsFromFrameStructureStart* in 250 ns resolution.  The total time since the particular frame structure start is *secondsFromFrameStructureStart + fractionalSecondsFromFrameStructureStart* |
| ***frameDrift***  This field specifies the drift rate of the GNSS‑network time relation with scale factor 2-30 seconds/second, in the range from ‑5.9605e-8 to +5.8673e-8 sec/sec. |
| ***cellID***  This field specifies the cell for which the GNSS–network time relation is provided. |
| ***physCellId***  This field specifies the physical cell identity of the reference cell (E-UTRA), as defined in TS 36.331 [12], for which the GNSS network time relation is provided. |
| ***cellGlobalIdEUTRA***  This field specifies the Evolved Cell Global Identifier (ECGI), the globally unique identity of a cell in E-UTRA, of the reference cell for the GNSS‑network time relation, as defined in TS 36.331 [12]. |
| ***earfcn***  This field specifies E-ARFCN of the reference cell for the GNSS‑network time relation (E-UTRA). In the case the server includes *earfcn-v9a0*, the server shall set the corresponding *earfcn* (i.e. without suffix) to *maxEARFCN*. |
| ***primary-CPICH-Info***  This field specifies the physical cell identity of the reference cell (UTRA) for the GNSS‑network time relation, as defined in TS 25.331 [13]. |
| ***cellParameters***  This field specifies the physical cell identity of the reference cell (UTRA) for the GNSS‑network time relation, as defined in TS 25.331 [13]. |
| ***cellGlobalIdUTRA***  The field specifies the global UTRAN Cell Identifier, the globally unique identity of a cell in UTRA, of the reference cell for the GNSS‑network time relation, as defined in TS 25.331 [13]. |
| ***uarfcn***  This field specifies ARFCN of the reference cell for the GNSS‑network time relation (UTRA). |
| ***bcchCarrier***  This field specifies the absolute GSM RF channel number of the BCCH of the reference base station (GERAN) for the GNSS‑network time relation, as defined in TS 44.031 [14]. |
| ***bsic***  This field specifies the Base Station Identity Code of the reference base station (GERAN) for the GNSS‑network time relation, as defined in TS 44.031 [14]. |
| ***cellGlobalIdGERAN***  This field specifies the Cell Global Identification (CGI), the globally unique identity of a cell in GERAN, of the reference base station for the GNSS‑network time relation. |
| ***nbPhysCellId***  This field specifies the narrowband physical layer cell identity of the NB-IoT reference cell, as defined in TS 36.331 [12], for which the GNSS network time relation is provided. |
| ***nbCellGlobalId***  This field specifies the global cell identifier of the NB-IoT reference cell for which the GNSS‑network time relation is provided, as defined in TS 36.331 [12]. |
| ***nbCarrierFreq***  This field specifies the carrier frequency of the NB-IoT reference cell for which the GNSS‑network time relation is provided. |
| ***nrPhysCellId***  This field specifies the physical cell identity of the reference cell (NR), as defined in TS 38.331 [35], for which the GNSS network time relation is provided. |
| ***nrCellGlobalID***  This field specifies the NR Cell Global Identifier (NCGI) of the reference cell (NR) for the GNSS‑network time relation, as defined in TS 38.331 [35]. |
| ***nrARFCN***  This field specifies NR-ARFCN of the reference cell (NR) for the GNSS‑network time relation. |

#### – *GNSS-ReferenceLocation*

The IE *GNSS-ReferenceLocation* is used by the location server to provide the target device with a‑priori knowledge of its location in order to improve GNSS receiver performance. The IE *GNSS-ReferenceLocation* is provided in WGS‑84 reference system.

-- ASN1START

GNSS-ReferenceLocation ::= SEQUENCE {

threeDlocation EllipsoidPointWithAltitudeAndUncertaintyEllipsoid,

...

}

-- ASN1STOP

#### – *GNSS-IonosphericModel*

The IE *GNSS-IonosphericModel* is used by the location server to provide parameters to model the propagation delay of the GNSS signals through the ionosphere. Proper use of these fields allows a single‑frequency GNSS receiver to remove parts of the ionospheric delay from the pseudorange measurements. Three Ionospheric Models are supported: The Klobuchar model as defined in [4], the NeQuick model as defined in [8] , and the klobucharModel2 as defined in [39].

-- ASN1START

GNSS-IonosphericModel ::= SEQUENCE {

klobucharModel KlobucharModelParameter OPTIONAL, -- Need ON

neQuickModel NeQuickModelParameter OPTIONAL, -- Need ON

...,

[[ klobucharModel2-r16 KlobucharModel2Parameter-r16 OPTIONAL -- Need ON

]]

}

-- ASN1STOP

#### – *KlobucharModelParameter*

-- ASN1START

KlobucharModelParameter ::= SEQUENCE {

dataID BIT STRING (SIZE (2)),

alfa0 INTEGER (-128..127),

alfa1 INTEGER (-128..127),

alfa2 INTEGER (-128..127),

alfa3 INTEGER (-128..127),

beta0 INTEGER (-128..127),

beta1 INTEGER (-128..127),

beta2 INTEGER (-128..127),

beta3 INTEGER (-128..127),

...

}

-- ASN1STOP

| *KlobucharModelParamater* field descriptions |
| --- |
| ***dataID***  When *dataID* has the value ′11′ it indicates that the parameters have been generated by QZSS, and the parameters have been specialized and are applicable within the area defined in [7]. When *dataID* has the value ′01′ it indicates that the parameters have been generated by BDS, and UE shall use these parameters according to the description given in 5.2.4.7 in [23], [50]. When the *dataID* has the value ′10′, it indicates that the parameters have been generated by NavIC, and UE shall use these parameters according to the description given in [38]. When *dataID* has the value ′00′ it indicates the parameters are applicable worldwide [4], [7]. |
| ***alfa0***  This field specifies the 0 parameter of the Klobuchar model, as specified in [4], [23], [38], [50].  Scale factor 2-30 seconds. |
| ***alfa1***  This field specifies the 1 parameter of the Klobuchar model, as specified in [4], [23], [38], [50].  Scale factor 2-27 seconds/semi-circle. |
| ***alfa2***  This field specifies the 2 parameter of the Klobuchar model, as specified in [4], [23], [38], [50].  Scale factor 2-24 seconds/semi-circle2. |
| ***alfa3***  This field specifies the 3 parameter of the Klobuchar model, as specified in [4], [23], [38], [50].  Scale factor 2-24 seconds/semi-circle3. |
| ***beta0***  This field specifies the 0 parameter of the Klobuchar model, as specified in [4], [23], [38], [50].  Scale factor 211 seconds. |
| ***beta1***  This field specifies the 1 parameter of the Klobuchar model, as specified in [4], [23], [38], [50].  Scale factor 214 seconds/semi-circle. |
| ***beta2***  This field specifies the 2 parameter of the Klobuchar model, as specified in [4], [23], [38, [50].  Scale factor 216 seconds/semi-circle2. |
| ***beta3***  This field specifies the 3 parameter of the Klobuchar model, as specified in [4], [23], [38], [50].  Scale factor 216 seconds/semi-circle3. |

#### – *KlobucharModel2Parameter*

-- ASN1START

KlobucharModel2Parameter-r16 ::= SEQUENCE {

alfa1-r16 INTEGER (0..1023),

alfa2-r16 INTEGER (-128..127),

alfa3-r16 INTEGER (0..255),

alfa4-r16 INTEGER (0..255),

alfa5-r16 INTEGER (0..255),

alfa6-r16 INTEGER (-128..127),

alfa7-r16 INTEGER (-128..127),

alfa8-r16 INTEGER (-128..127),

alfa9-r16 INTEGER (-128..127),

...

}

-- ASN1STOP

| *KlobucharModel2Parameter* field descriptions |
| --- |
| ***alfa1***  This field specifies the 1 parameter of the Klobuchar model, as specified in 7.8.1 in [39], [49].  Scale factor 2-3 TECU. |
| ***alfa2***  This field specifies the 2 parameter of the Klobuchar model, as specified in 7.8.1 in [39], [49].  Scale factor 2-3 TECU. |
| ***alfa3***  This field specifies the 3 parameter of the Klobuchar model, as specified in 7.8.1 in [39], [49].  Scale factor 2-3 TECU. |
| ***alfa4***  This field specifies the 4 parameter of the Klobuchar model, as specified in 7.8.1 in [39], [49].  Scale factor 2-3 TECU. |
| ***alfa5***  This field specifies the  parameter of the Klobuchar model, as specified in 7.8.1 in [39], [49].  Scale factor -2-3 TECU. |
| ***alfa6***  This field specifies the 6 parameter of the Klobuchar model, as specified in 7.8.1 in [39], [49].  Scale factor 2-3 TECU. |
| ***alfa7***  This field specifies the 7 parameter of the Klobuchar model, as specified in 7.8.1 in [39], [49].  Scale factor 2-3 TECU. |
| ***alfa8***  This field specifies the 8 parameter of the Klobuchar model, as specified in 7.8.1 in [39], [49].  Scale factor 2-3 TECU. |
| ***alfa9***  This field specifies the 9 parameter of the Klobuchar model, as specified in 7.8.1 in [39], [49].  Scale factor 2-3 TECU. |

#### – *NeQuickModelParameter*

-- ASN1START

NeQuickModelParameter ::= SEQUENCE {

ai0 INTEGER (0..2047),

ai1 INTEGER (-1024..1023),

ai2 INTEGER (-8192..8191),

ionoStormFlag1 INTEGER (0..1) OPTIONAL, -- Need OP

ionoStormFlag2 INTEGER (0..1) OPTIONAL, -- Need OP

ionoStormFlag3 INTEGER (0..1) OPTIONAL, -- Need OP

ionoStormFlag4 INTEGER (0..1) OPTIONAL, -- Need OP

ionoStormFlag5 INTEGER (0..1) OPTIONAL, -- Need OP

...

}

-- ASN1STOP

| *NeQuickModelParameter* field descriptions |
| --- |
| ***ai0***  Effective Ionisation Level 1st order parameter.  Scale factor 2-2 Solar Flux Units (SFUs), [8] clause 5.1.6. |
| ***ai1***  Effective Ionisation Level 2nd order parameter.  Scale factor 2-8 Solar Flux Units/degree, [8] clause 5.1.6. |
| ***ai2***  Effective Ionisation Level 3rd order parameter.  Scale factor 2-15 Solar Flux Units/degree2, [8] clause 5.1.6. |
| ***ionoStormFlag1, ionoStormFlag2, ionoStormFlag3, ionoStormFlag4, ionoStormFlag5***  These fields specify the ionosphere disturbance flags (1,…,5) for five different regions as described in [8], clause 5.1.6. If the ionosphere disturbance flag for a region is not present the target device shall treat the ionosphere disturbance condition as unknown. |

#### – *GNSS-EarthOrientationParameters*

The IE *GNSS-EarthOrientationParameters* is used by the location server to provide parameters to construct the ECEF and ECI coordinate transformation as defined in [4]. The IE *GNSS-EarthOrientationParameters* indicates the relationship between the Earth′s rotational axis and WGS-84 reference system.

-- ASN1START

GNSS-EarthOrientationParameters ::= SEQUENCE {

teop INTEGER (0..65535),

pmX INTEGER (-1048576..1048575),

pmXdot INTEGER (-16384..16383),

pmY INTEGER (-1048576..1048575),

pmYdot INTEGER (-16384..16383),

deltaUT1 INTEGER (-1073741824..1073741823),

deltaUT1dot INTEGER (-262144..262143),

...

}

-- ASN1STOP

| *GNSS-EarthOrientationParameters* field descriptions |
| --- |
| ***teop***  This field specifies the EOP data reference time in seconds, as specified in [4], [39].  Scale factor 24 seconds. |
| ***pmX***  This field specifies the X-axis polar motion value at reference time in arc-seconds, as specified in [4], [39], [49].  Scale factor 2-20 arc-seconds. |
| ***pmXdot***  This field specifies the X-axis polar motion drift at reference time in arc-seconds/day, as specified in [4], [39], [49].  Scale factor 2-21 arc-seconds/day. |
| ***pmY***  This field specifies the Y-axis polar motion value at reference time in arc-seconds, as specified in [4], [39], [49].  Scale factor 2-20 arc-seconds. |
| ***pmYdot***  This field specifies the Y-axis polar motion drift at reference time in arc-seconds/day, as specified in [4], [39], [49].  Scale factor 2-21 arc-seconds/day. |
| ***deltaUT1***  This field specifies the UT1-UTC difference at reference time in seconds, as specified in [4], [39], [49].  Scale factor 2-24 seconds. |
| ***deltaUT1dot***  This field specifies the Rate of UT1-UTC difference at reference time in seconds/day, as specified in [4], [39], [49]  Scale factor 2-25 seconds/day. |

#### *– GNSS-RTK-ReferenceStationInfo*

The IE *GNSS-RTK-ReferenceStationInfo* is used by the location server to provide the Earth-centered, Earth-fixed (ECEF) coordinates of the antenna reference point (ARP) of the stationary reference station for which the *GNSS‑RTK‑Observations* assistance data are provided together with reference station antenna description.

The parameters provided in IE *GNSS-RTK-ReferenceStationInfo* are used as specified for message type 1006, 1033 and 1032 in [30].

-- ASN1START

GNSS-RTK-ReferenceStationInfo-r15 ::= SEQUENCE {

referenceStationID-r15 GNSS-ReferenceStationID-r15,

referenceStationIndicator-r15 ENUMERATED {physical, non-physical},

antenna-reference-point-ECEF-X-r15 INTEGER (-137438953472..137438953471),

antenna-reference-point-ECEF-Y-r15 INTEGER (-137438953472..137438953471),

antenna-reference-point-ECEF-Z-r15 INTEGER (-137438953472..137438953471),

antennaHeight-r15 INTEGER (0..65535) OPTIONAL, -- Need ON

antennaDescription-r15 AntennaDescription-r15 OPTIONAL, -- Need ON

antenna-reference-point-unc-r15 AntennaReferencePointUnc-r15 OPTIONAL, -- Need ON

physical-reference-station-info-r15 PhysicalReferenceStationInfo-r15 OPTIONAL, -- Cond NP

...,

[[

equalIntegerAmbiguityLevel-r16 EqualIntegerAmbiguityLevel-r16 OPTIONAL -- Need ON

]]

}

AntennaDescription-r15 ::= SEQUENCE {

antennaDescriptor-r15 VisibleString (SIZE (1..256)),

antennaSetUpID-r15 ENUMERATED { non-zero } OPTIONAL, -- Need OP

...

}

AntennaReferencePointUnc-r15 ::= SEQUENCE {

uncertainty-X-r15 INTEGER (0..255),

confidence-X-r15 INTEGER (0..100),

uncertainty-Y-r15 INTEGER (0..255),

confidence-Y-r15 INTEGER (0..100),

uncertainty-Z-r15 INTEGER (0..255),

confidence-Z-r15 INTEGER (0..100),

...

}

PhysicalReferenceStationInfo-r15 ::= SEQUENCE {

physicalReferenceStationID-r15 GNSS-ReferenceStationID-r15,

physical-ARP-ECEF-X-r15 INTEGER (-137438953472..137438953471),

physical-ARP-ECEF-Y-r15 INTEGER (-137438953472..137438953471),

physical-ARP-ECEF-Z-r15 INTEGER (-137438953472..137438953471),

physical-ARP-unc-r15 AntennaReferencePointUnc-r15 OPTIONAL, -- Need ON

...

}

EqualIntegerAmbiguityLevel-r16 ::= CHOICE {

allReferenceStations-r16 NULL,

referenceStationList-r16 ReferenceStationList-r16

}

ReferenceStationList-r16 ::= SEQUENCE (SIZE(1..16)) OF GNSS-ReferenceStationID-r15

-- ASN1STOP

| Conditional presence | Explanation |
| --- | --- |
| *NP* | The field is optionally present, need ON, if the *referenceStationIndicator* has the value ′*non-physical*′; otherwise it is not present. |

| *GNSS-RTK-ReferenceStationInfo* field descriptions |
| --- |
| ***referenceStationID***  The Reference Station ID is determined by the RTK service provider. |
| ***referenceStationIndicator***  This fields specifies type of reference station. Enumerated value *physical* indicates a real, physical reference station; value *non-physical* indicates a non-physical or computed reference station. |
| ***antenna-reference-point-ECEF-X***  This field specifies the antenna reference point X-coordinate in the World Geodetic System 1984 (WGS 84) datum.  Scale factor 0.0001 m; range ±13,743,895.3471 m. |
| ***antenna-reference-point-ECEF-Y***  This field specifies the antenna reference point Y-coordinate in the World Geodetic System 1984 (WGS 84) datum.  Scale factor 0.0001 m; range ±13,743,895.3471 m. |
| ***antenna-reference-point-ECEF-Z***  This field specifies the antenna reference point Z-coordinate in the World Geodetic System 1984 (WGS 84) datum.  Scale factor 0.0001 m; range ±13,743,895.3471 m. |
| ***antennaHeight***  This field specifies the height of the Antenna Reference Point above the marker used in the survey campaign.  Scale factor 0.0001 m; range 0–6.5535 m. |
| ***antennaDescriptor***  This field provides an ASCII descriptor of the reference station antenna using IGS naming convention [31]. The descriptor can be used to look up model specific phase centre corrections of that antenna. |
| ***antennaSetUpID***  This field, if present, indicates that the standard IGS Model is not valid (≠ 0 [30]). If this field is absent the standard IGS Model is valid (′0 = Use standard IGS Model′ [30]). |
| ***antenna-reference-point-unc***  This field specifies the uncertainty of the ARP coordinates. *uncertainty-X*, *uncertainty-Y*, and *uncertainty-Z* correspond to the encoded high accuracy uncertainty of the X, Y, and Z-coordinate, respectively, as defined in TS 23.032 [15]. *confidence-X*, *confidence-Y*, and *confidence-Z* corresponds to confidence as defined in TS 23.032 [15]. |
| ***physical-reference-station-info***  This field provides the earth-centred, earth-fixed (ECEF) coordinates of the antenna reference point (ARP) for the real (or "physical") reference station used. This field may be used in the case of the non-physical reference station approach to allow the target device to refer baseline vectors to a physical reference rather than to a non-physical reference without any connection to a physical point. |
| ***physicalReferenceStationID***  This field specifies the station ID of a real reference station, when the *referenceStationIndicator* has the value ′*non-physical*′. |
| ***physical-ARP-ECEF-X***  This field specifies the antenna reference point X-coordinate in the World Geodetic System 1984 (WGS 84) datum.  Scale factor 0.0001 m; range ±13,743,895.3471 m. |
| ***physical-ARP-ECEF-Y***  This field specifies the antenna reference point Y-coordinate in the World Geodetic System 1984 (WGS 84) datum.  Scale factor 0.0001 m; range ±13,743,895.3471 m. |
| ***physical-ARP-ECEF-Z***  This field specifies the antenna reference point Z-coordinate in the World Geodetic System 1984 (WGS 84) datum.  Scale factor 0.0001 m; range ±13,743,895.3471 m. |
| ***physical-ARP-unc***  This field specifies the uncertainty of the ARP coordinates. |
| ***equalIntegerAmbiguityLevel***  This field specifies the integer ambiguity level of this reference station in relation to other reference stations. Either, the presence or absence of *allReferenceStations* indicates whether the integer ambiguity level may be assumed to be aligned between all reference stations or not (interpreted as no alignment is facilitated from the location server), or *referenceStationList* provides a list of reference stations for which the integer ambiguity level may be assumed to be the same. | |

#### *– GNSS-RTK-CommonObservationInfo*

The IE *GNSS-RTK-CommonObservationInfo* is used by the location server to provide common information applicable to the IE *GNSS-RTK-Observations.*

The parameters provided in IE *GNSS-RTK-CommonObservationInfo* are used as specified for message type 1071-1127 in [30].

-- ASN1START

GNSS-RTK-CommonObservationInfo-r15 ::= SEQUENCE {

referenceStationID-r15 GNSS-ReferenceStationID-r15,

clockSteeringIndicator-r15 INTEGER (0..3),

externalClockIndicator-r15 INTEGER (0..3),

smoothingIndicator-r15 BIT STRING (SIZE(1)),

smoothingInterval-r15 BIT STRING (SIZE(3)),

...

}

-- ASN1STOP

| *GNSS-RTK-CommonObservationInfo* field descriptions |
| --- |
| ***referenceStationID***  This field specifies the Station ID for which the *GNSS-RTK-Observations* are provided. |
| ***clockSteeringIndicator***  This field provides the clock steering indicator. The interpretation of the value is as follows:  0 clock steering is not applied  In this case, the receiver clock must be kept in the range of ±1 ms (approximately ±300 km)  1 clock steering has been applied  In this case, the receiver clock must be kept in the range of ±1 microsecond (approximately ±300 metres).  2 unknown clock steering status  3 reserved |
| ***externalClockIndicator***  This field provides the external clock indicator. The interpretation of the value is as follows:  0 internal clock is used  1 external clock is used, clock status is "locked"  2 external clock is used, clock status is "not locked", which may indicate external clock failure and that the transmitted data may not be reliable.  3 unknown clock is used |
| ***smoothingIndicator***  This field provides the GNSS Divergence-free Smoothing Indicator. The interpretation of the value is as follows:  1 Divergence-free smoothing is used  0 Other type of smoothing is used |
| ***smoothingInterval***  The GNSS Smoothing Interval is the integration period over which the pseudorange code phase measurements are averaged using carrier phase information. Divergence-free smoothing may be continuous over the entire period for which the satellite is visible. A value of zero indicates no smoothing is used.  See table "*smoothingInterval* value to Smoothing Interval relation" below. |

*smoothingInterval* value to Smoothing Interval relation

|  |  |
| --- | --- |
| *smoothingInterval* value | Smoothing Interval |
| 000 (0) | No smoothing |
| 001 (1) | < 30 s |
| 010 (2) | 30-60 s |
| 011 (3) | 1-2 min |
| 100 (4) | 2-4 min |
| 101 (5) | 4-8 min |
| 110 (6) | >8 min |
| 111 (7) | Unlimited smoothing interval |

#### *– GNSS-RTK-AuxiliaryStationData*

The IE *GNSS-RTK-AuxiliaryStationData* is used by the location server to provide the coordinates of the antenna reference point (ARP) of Auxiliary Reference Stations, relative to the coordinates provided in IE *GNSS‑RTK‑ReferenceStationInfo*. The reference station provided in IE *GNSS-RTK-ReferenceStationInfo* is the Master Reference Station. Therefore, one Master Reference Station with its associated Auxiliary Stations is used in a single Provide Assistance Data message.

The parameters provided in IE *GNSS-RTK-AuxiliaryStationData* are used as specified for message type 1014 in [30].

-- ASN1START

GNSS-RTK-AuxiliaryStationData-r15 ::= SEQUENCE {

networkID-r15 GNSS-NetworkID-r15,

subNetworkID-r15 GNSS-SubNetworkID-r15 OPTIONAL, -- Need ON

master-referenceStationID-r15 GNSS-ReferenceStationID-r15,

auxiliaryStationList-r15 AuxiliaryStationList-r15,

...

}

AuxiliaryStationList-r15 ::= SEQUENCE (SIZE (1..32)) OF AuxiliaryStationElement-r15

AuxiliaryStationElement-r15 ::= SEQUENCE {

aux-referenceStationID-r15 GNSS-ReferenceStationID-r15,

aux-master-delta-latitude-r15 INTEGER (-524288..524287),

aux-master-delta-longitude-r15 INTEGER (-1048576..1048575),

aux-master-delta-height-r15 INTEGER (-4194304..4194303),

aux-ARP-unc-r15 Aux-ARP-Unc-r15 OPTIONAL, -- Need ON

...

}

Aux-ARP-Unc-r15 ::= SEQUENCE {

horizontalUncertainty-r15 INTEGER (0..255),

horizontalConfidence-r15 INTEGER (0..100),

verticalUncertainty-r15 INTEGER (0..255) OPTIONAL, -- Need ON

verticalConfidence-r15 INTEGER (0..100) OPTIONAL, -- Need ON

...

}

-- ASN1STOP

| *GNSS-RTK-AuxiliaryStationData* field descriptions |
| --- |
| ***networkID***  This field defines the network and the source of the particular set of reference stations and their observation information. The RTK service provider should ensure that the *networkID* is unique in the region serviced. The *networkID* indicates an area and its reference stations where the service providers will provide a homogenous solution with levelled integer ambiguities between its reference stations. In general, the area indicated by *networkID* will comprise one subnetwork with a unique *subNetworkID*. |
| ***subNetworkID***  This field identifies the subnetwork of a network identified by *networkID*. In general the area indicated by *networkID* will consist of one subnetwork. The *subNetworkID* indicates the actual solution number of integer ambiguity level. If one network has only one subnetwork, this indicates that an ambiguity level throughout the whole network is established. |
| ***master-referenceStationID***  This field identifies the Master Reference Station. |
| ***aux-referenceStationID***  This field identifies the Auxiliary Reference Station. |
| ***aux-master-delta-latitude***  This field provides the delta value in latitude of Antenna Reference Point of "Auxiliary Reference Station minus Master Reference Station" in geographical coordinates based on GRS80 ellipsoid parameters for the same ECEF system as used in IE *GNSS‑RTK‑ReferenceStationInfo*.  Scale factor 25×10-6 degrees; range ±13.1071 degrees. |
| ***aux-master-delta-longitude***  This field provides the delta value in longitude of Antenna Reference Point of "Auxiliary Reference Station minus Master Reference Station" in geographical coordinates based on GRS80 ellipsoid parameters for the same ECEF system as used in IE *GNSS‑RTK‑ReferenceStationInfo*.  Scale factor 25×10-6 degrees; range ±26.2142 degrees. |
| ***aux-master-delta-height***  This field provides the delta value in ellipsoidal height of Antenna Reference Point of "Auxiliary Reference Station minus Master Reference Station" in geographical coordinates based on GRS80 ellipsoid parameters for the same ECEF system as used in IE *GNSS‑RTK‑ReferenceStationInfo*.  Scale factor 1 millimetre; range ±4194.303 m. |
| ***aux-ARP-unc***  This field specifies the uncertainty of the auxiliary station ARP coordinates and comprise the following fields:  - ***horizontalUncertainty*** indicates the horizontal uncertainty of the ARP latitude/longitude. The ′*horizontalUncertainty*′ corresponds to the encoded high accuracy uncertainty as defined in TS 23.032 [15] and ′*horizontalConfidence*′ corresponds to confidence as defined in TS 23.032 [15].  - ***verticalUncertainty*** indicates the vertical uncertainty of the ARP altitude. The '*verticalUncertainty*' corresponds to the encoded high accuracy uncertainty as defined in TS 23.032 [15] and '*verticalConfidence*' corresponds to confidence as defined in TS 23.032 [15]. |

#### *– GNSS-SSR-CorrectionPoints*

The IE *GNSS-SSR-CorrectionPoints* is used by the location server to provide a list of correction point coordinates or an array of correction points ("grid") for which the *GNSS‑SSR‑GriddedCorrection* are valid.

-- ASN1START

GNSS-SSR-CorrectionPoints-r16 ::= SEQUENCE {

correctionPointSetID-r16 INTEGER (0..16383),

correctionPoints-r16 CHOICE {

listOfCorrectionPoints-r16 GNSS-SSR-ListOfCorrectionPoints-r16,

arrayOfCorrectionPoints-r16 GNSS-SSR-ArrayOfCorrectionPoints-r16

},

...

}

GNSS-SSR-ListOfCorrectionPoints-r16 ::= SEQUENCE {

referencePointLatitude-r16 INTEGER (-16384..16383),

referencePointLongitude-r16 INTEGER (-32768..32767),

relativeLocationsList-r16 SEQUENCE (SIZE (0..63)) OF RelativeLocationElement-r16,

...

}

RelativeLocationElement-r16 ::= SEQUENCE {

deltaLatitude-r16 INTEGER (-512..511),

deltaLongitude-r16 INTEGER (-1024..1023),

...

}

GNSS-SSR-ArrayOfCorrectionPoints-r16 ::=SEQUENCE {

referencePointLatitude-r16 INTEGER (-16384..16383),

referencePointLongitude-r16 INTEGER (-32768..32767),

numberOfStepsLatitude-r16 INTEGER (0..63),

numberOfStepsLongitude-r16 INTEGER (0..63),

stepOfLatitude-r16 INTEGER (1..511),

stepOfLongitude-r16 INTEGER (1..1023),

bitmaskOfGrids-r16 BIT STRING (SIZE(64)) OPTIONAL, -- Need OP

...

}

-- ASN1STOP

| *GNSS-SSR-CorrectionPoints* field descriptions |
| --- |
| ***correctionPointSetID***  This field provides the ID of the Atmospheric Correction Point set. It is a regionally unique arbitrary number that is used by the UE to ensure that the atmospheric corrections are being applied to the correct set of points. |
| ***referencePointLatitude***  This field specifies the latitude for the reference point, expressed in the range of -90° , +90°, coded as a number between -214 and 214-1, coded in 2's complement binary on 15 bits. The relation between the latitude X in the range [‑90°, 90°] and the coded number N is:    where  denotes the greatest integer less than or equal to x (floor operator).  For the *listOfCorrectionPoints*, the reference point defines the 1st correction point location.  For the *arrayOfCorrectionPoints*, the reference point defines the northwest corner of the correction point array. |
| ***referencePointLongitude***  This field specifies the longitude for the reference point, expressed in the range -180°, +180°, coded as a number between -215 and 215-1, coded in 2's complement binary on 16 bits. The relation between the longitude X in the range [-180°, 180°) and the coded number N is:    For the *listOfCorrectionPoints*, the reference point defines the 1st correction point location.  For the *arrayOfCorrectionPoints*, the reference point defines the northwest corner of the correction point array. |
| ***relativeLocationsList***  This field specifies the 2nd, 3rd, …, 64th correction point location. |
| ***deltaLatitude***  This field specifies the delta value in latitude of this correction point location relative to the previous point on the list or the reference point in the case of the first additional point, defined as "correction point location" minus "previous correction point location" in units of 0.01 degrees. |
| ***deltaLongitude***  This field specifies the delta value in longitude of this correction point location relative to the previous point on the list or the reference point in the case of the first additional point, defined as "correction point location" minus "previous correction point location" in units of 0.01 degrees. |
| ***numberOfStepsLatitude*, *numberOfStepsLongitude***  These fields specify the number of steps for latitude and longitude direction respectively. |
| ***stepOfLatitude, stepOfLongitude***  These fields specify the spacing of the correction points for latitude and longitude respectively. The unit and scale factor is 0.01 degrees. |
| ***bitmaskOfGrids***  This field specifies the availability of correction data at the correction points in the array. If a specific bit is enabled (set to '1'), the correction is available. Only the first (*numberOfStepsLatitude + 1)*×(*numberOfStepsLongitude + 1*) bits are used, the remainder are set to '0'. Starting with the northwest corner of the array (top left on a north oriented map) the correction points are enumerated with row precedence – first row west to east, second row west to east, until last row west to east – ending with the southeast corner of the array. If the field is omitted all correction points are used and none omitted. |

#### – *GNSS-Integrity-ServiceParameters*

The IE *GNSS-Integrity-ServiceParameters* is used by the location server to provide the range of Integrity Risk (IR) for which the GNSS integrity assistance data are valid.

-- ASN1START

GNSS-Integrity-ServiceParameters-r17 ::= SEQUENCE {

irMinimum-r17 INTEGER (0..255),

irMaximum-r17 INTEGER (0..255),

...

}

-- ASN1STOP

|  |
| --- |
| *GNSS-Integrity-ServiceParameters* field descriptions |
| ***irMinimum***  This field specifies the Minimum Integrity Risk (IR) which is the minimum IR for which the error bounds provided in the IEs *SSR-IntegrityOrbitBounds*, *SSR-IntegrityClockBounds*, *SSR-IntegrityCodeBiasBounds*, *SSR-IntegrityPhaseBiasBounds*, *STEC-IntegrityErrorBounds*, and *TropoDelayIntegrityErrorBounds* are valid.  The IR is calculated by where n is the value of *irMinimum* and the range is 10-10.2 to 1. |
| ***irMaximum***  This field specifies the Maximum Integrity Risk (IR) which is the maximum IR for which the error bounds provided in the IEs *SSR-IntegrityOrbitBounds*, *SSR-IntegrityClockBounds*, *SSR-IntegrityCodeBiasBounds*, *SSR-IntegrityPhaseBiasBounds*, *STEC-IntegrityErrorBounds*, and *TropoDelayIntegrityErrorBounds* are valid.  The IR is calculated by where n is the value of *irMaximum* and the range is 10-10.2 to 1. |

#### – *GNSS-Integrity-ServiceAlert*

The IE *GNSS-Integrity-ServiceAlert* is used by the location server to indicate whether the corresponding assistance data can be used for integrity related applications.

-- ASN1START

GNSS-Integrity-ServiceAlert-r17 ::= SEQUENCE {

ionosphereDoNotUse-r17 BOOLEAN,

troposphereDoNotUse-r17 BOOLEAN,

...

}

-- ASN1STOP

|  |
| --- |
| *GNSS-Integrity-ServiceAlert* field descriptions |
| ***ionosphereDoNotUse***  This field indicates whether the ionospheric corrections in IE *GNSS-SSR-STEC-Correction* can be used for integrity related applications (FALSE) or not (TRUE). |
| ***troposphereDoNotUse***  This field indicates whether the tropospheric corrections in IE *GNSS-SSR-GriddedCorrection* can be used for integrity related applications (FALSE) or not (TRUE). |

#### – *GNSS-LOS-NLOS-GridPoints*

The IE *GNSS-LOS-NLOS-GridPoints* is used by the location server to provide a list of grid point coordinates or an array of correction points ("grid") for which specific assistance data can be provided.

-- ASN1START

GNSS-LOS-NLOS-GridPoints-r18 ::= SEQUENCE {

gridPointsSetID-r18 INTEGER (0..16383),

horizontalGridPoints-r18 ArrayOfGridPoints-r18,

referenceAltitudeFine-r18 INTEGER (0..9) OPTIONAL, -- Need OP

verticalGridPoints-r18 VerticalGridPoints-r18 OPTIONAL, -- Cond 3D

...

}

ArrayOfGridPoints-r18 ::= SEQUENCE {

referencePointLatitude-r18 INTEGER (-16777216.. 16777215),

referencePointLongitude-r18 INTEGER (-33554432.. 33554431),

numberOfStepsSouth-r18 INTEGER (0.. 255),

numberOfStepsEast-r18 INTEGER (0.. 255),

stepSouth-r18 SpatialDelta-r18,

stepEast-r18 SpatialDelta-r18,

bitmaskOfGrids-r18 CHOICE {

bog16-r18 BIT STRING (SIZE(16)),

bog64-r18 BIT STRING (SIZE(64)),

bog256-r18 BIT STRING (SIZE(256)),

...

} OPTIONAL, -- Need OP

...

}

VerticalGridPoints-r18 ::=SEQUENCE {

referenceAltitudeCoarse-r18 INTEGER (-50..900),

numberOfStepsDown-r18 INTEGER (1..3),

stepDown-r18 SpatialDelta-r18,

upperValidityDeltaAltitude-r18 SpatialDelta-r18 OPTIONAL, -- Need OP

lowerValidityDeltaAltitude-r18 SpatialDelta-r18 OPTIONAL, -- Need OP

...

}

SpatialDelta-r18 ::= ENUMERATED {n1, n2, n3, n4, n5, n10, n20, n50, n100}

-- ASN1STOP

| Conditional presence | Explanation |
| --- | --- |
| *3D* | This field is mandatory present if a 3D grid is provided; otherwise it is absent. |

| *GNSS-LOS-NLOS-GridPoints* field descriptions |
| --- |
| ***gridPointsSetID***  This field provides the ID of the spatial grid point set. It is a regionally unique arbitrary number that is used by the UE to ensure that provided assistance data associated to a spatial grid point set is being applied to the correct set of points.  The grid point set ID identifies a grid defined by a reference point corresponding to the northwest corner (of the upper layer in case of a 3D grid), where the rest of the grid is defined by a number of steps and step lengths in the south, east (down in case of a 3D grid). The grid is valid within the horizontal perimeter of the grid and between an upper and lower validity altitude, where the upper validity altitude is (*referenceAltitudeFine* + 10\* *referenceAltitudeCoarse* + *upperValidityDeltaAltitude*), and the lower validity altitude is (*referenceAltitudeFine* + 10\* *referenceAltitudeCoarse* – *numberOfStepsDown*\**stepDown* – *lowerValidityDeltaAltitude*). |
| ***referencePointLatitude***  This field specifies the latitude for the reference point, expressed in the range of -90° , +90°, coded as a number between -224 and 224-1, coded in 2's complement binary on 25 bits. The relation between the latitude X in the range [‑90°, 90°] and the coded number N is:    where  denotes the greatest integer less than or equal to x (floor operator).  The reference point defines the northwest corner of the grid point array. |
| ***referencePointLongitude***  This field specifies the longitude for the reference point, expressed in the range -180°, +180°, coded as a number between -225 and 225-1, coded in 2's complement binary on 26 bits. The relation between the longitude X in the range [-180°, 180°) and the coded number N is:    The reference point defines the northwest corner of the grid point array. |
| ***numberOfStepsSouth, numberOfStepsEast, numberOfStepsDown***  These fields specify the number of steps for south, east and down direction respectively. |
| ***stepSouth, stepEast, stepDown***  These fields specify the spacing of the grid points for south, east and down respectively. Enumerated values *n1, n2, n3, n4, n5, n10, n20, n50, n100* correspond to 1, 2, 3, 4, 5, 10, 20, 50, 100 meters, respectively. |
| ***bitmaskOfGrids***  This field specifies the availability of grid data at the horizontal grid points in the array and applies to all altitude layers of the grid. If a specific bit is enabled (set to '1'), the grid is available. Only the first (*numberOfStepsSouth*+1)×(*numberOfStepsEast*+1) bits are used, the remainder are set to '0'. Starting with the northwest corner of the array (top left on a north oriented map) the grid points are enumerated with row precedence – first row west to east, second row west to east, until last row west to east – ending with the southeast corner of the array. If the field is omitted all grid points are used and none omitted. |
| ***referenceAltitudeFine***  If this field is present and  - the field *referenceAltitudeCoarse* is also present, it provides the fine resolution of the 3D grid altitude of the upmost layer, or  - the field *referenceAltitudeCoarse* is absent, it provides the altitude above ground level of the 2D grid,  with a scale factor of 1m.  If the field is absent, the default value is 0m. |
| ***referenceAltitudeCoarse***  This field is present if a 3D grid is provided and specifies the coarse altitude, scale factor 10m, of the upmost layer of the grid relative to the WGS84 ellipsoid. If this field is absent, a 2D grid is provided, valid for ground level. |
| ***upperValidityDeltaAltitude***  This field, if present, specifies the upper validity altitude relative to the grid upper layer altitude. Enumerated values *n1, n2, n3, n4, n5, n10, n20, n50, n100* correspond to 1, 2, 3, 4, 5, 10, 20, 50, 100 meters, respectively. If the field is absent, the default value is 0m. |
| ***lowerValidityDeltaAltitude***  This field, if present, specifies the lower validity altitude relative to the lowest grid layer altitude. Enumerated values *n1, n2, n3, n4, n5, n10, n20, n50, n100* correspond to 1, 2, 3, 4, 5, 10, 20, 50, 100 meters, respectively. If the field is absent, the default value is 0m. |

#### *– GNSS-SSR-IOD-Update*

The IE *GNSS-SSR-IOD-Update* is used to indicate the Issue of Data (IOD) values of other IEs that are infrequently updated. The IEs with a matching IOD are linked and valid while the *GNSS-SSR-IOD-Update* is valid, i.e. during the *GNSS-SSR-IOD-Update* and *ssrUpdateInterval* and with respect to the *iod-ssr*.

-- ASN1START

GNSS-SSR-IOD-Update-r18 ::= SEQUENCE {

epochTime-r18 GNSS-SystemTime,

ssrUpdateInterval-r18 INTEGER (0..15),

iod-ssr-r18 INTEGER (0..15),

iod-ssr-PCVResiduals-r18 INTEGER (0..64),

...

}

-- ASN1STOP

| *GNSS-SSR-IOD-Update* field descriptions |
| --- |
| ***epochTime***  This field specifies the epoch time of validity of the information elements referenced via IOD values from this IE. The *gnss-TimeID* in *GNSS-SystemTime* shall be the same as the *GNSS-ID* in IE *GNSS-GenericAssistDataElement*. |
| ***ssrUpdateInterval***  This field specifies the SSR Update Interval. The SSR Update Intervals for all SSR parameters start at time 00:00:00 of the GPS time scale. A change of the SSR Update Interval during the transmission of SSR data should ensure consistent data for a target device. See table Value of *ssrUpdateInterval* to SSR Update Interval relation in IE *GNSS‑SSR‑OrbitCorrections*. |
| ***iod-ssr***  This field specifies the Issue of Data number for the SSR data. A change of *iod-ssr* is used to indicate a change in the SSR generating configuration. |
| ***iod-ssr-PCVResiduals***  This field specifies the Issue of Data for the SSR Satellite PCV Residuals that is valid while the *GNSS-SSR-IOD-Update* is valid. |

#### – *GNSS-TimeModelList*

The IE *GNSS-TimeModelList* is used by the location server to provide the GNSS‑GNSS system time offset between the GNSS system time indicated by IE *GNSS‑ID* in IE *GNSS-GenericAssistDataElement* to the GNSS system time indicated by IE *gnss-TO-ID*. Several *GNSS-TimeModelElement* IEs can be included with different *gnss-TO-ID* fields. The location server should provide a *GNSS-TimeModelList* for the same *GNSS-ID* as the *gnss-TimeID* in IE *GNSS-SystemTime* in *GNSS-ReferenceTime* assistance. If the location server does not provide a *GNSS-TimeModelList* for the same *GNSS-ID* as the *gnss-TimeID* in IE *GNSS-SystemTime* in *GNSS-ReferenceTime* assistance the target device assumes *tA1* and *tA2* are equal to zero.

-- ASN1START

GNSS-TimeModelList ::= SEQUENCE (SIZE (1..15)) OF GNSS-TimeModelElement

GNSS-TimeModelElement ::= SEQUENCE {

gnss-TimeModelRefTime INTEGER (0..65535),

tA0 INTEGER (-67108864..67108863),

tA1 INTEGER (-4096..4095) OPTIONAL, -- Need ON

tA2 INTEGER (-64..63) OPTIONAL, -- Need ON

gnss-TO-ID INTEGER (1..15),

weekNumber INTEGER (0..8191) OPTIONAL, -- Need ON

deltaT INTEGER (-128..127) OPTIONAL, -- Need ON

...

}

-- ASN1STOP

| *GNSS-TimeModelElement* field descriptions |
| --- |
| ***gnss-TimeModelRefTime***  This field specifies the reference time of week for *GNSS-TimeModelElement* and it is given in GNSS specific system time.  Scale factor 24 seconds. |
| ***tA0***  This field specifies the bias coefficient of the *GNSS-TimeModelElement*.  Scale factor 2-35 seconds. |
| ***tA1***  This field specifies the drift coefficient of the *GNSS-TimeModelElement.*  Scale factor of 2-51 seconds/second. |
| ***tA2***  This field specifies the drift rate correction coefficient of the *GNSS-TimeModelElement.*  Scale factor of 2-68 seconds/second2. |
| ***gnss-TO-ID***  This field specifies the GNSS system time of the GNSS for which the *GNSS-TimeModelElement* is applicable. *GNSS-TimeModelElement* contains parameters to convert GNSS system time from the system indicated by *GNSS‑ID* to GNSS system time indicated by *gnss-TO-ID*. The conversion is defined in [4,5,6]. See table of *gnss-TO-ID* to Indication relation below. NOTE. |
| ***weekNumber***  This field specifies the reference week of the *GNSS-TimeModelElement* given in GNSS specific system time. The location server should include this field, if *tA1* or *tA2* is included.  Scale factor 1 week. |
| ***deltaT***  This field specifies the integer number of seconds of the GNSS-GNSS time offset provided in the *GNSS-TimeModelElement.*  Scale factor 1 second. |

*gnss-TO-ID* to Indication relation

|  |  |
| --- | --- |
| Value of *gnss-TO-ID* | Indication |
| 1 | GPS |
| 2 | Galileo |
| 3 | QZSS |
| 4 | GLONASS |
| 5 | BDS |
| 6 | NavIC |
| 7-15 | reserved |

NOTE: The time relationship between the system time indicated by *GNSS-ID* and system time indicated by *gnss‑TO-ID* is given by the following equation:  
  
tGNSS = tE - ( A0GGTO + A1GGTO (tE - tGGTO + 604800 (WN - WNGGTO)) + A2GGTO (tE - tGGTO +   
 604800 (WN - WNGGTO))2 )  
  
where  
  
tGNSS  is the system time of week for the GNSS indicated by *gnss-TO-ID*.  
tE is the system time of week for the GNSS indicated by *GNSS-ID*.  
WN is the week number of the GNSS system time indicated by *GNSS-ID* corresponding to the tE.   
tGGTO is the system time of week for the time model data in the GNSS time indicated by *GNSS-ID* and given by the *gnss‑TimeModelRefTime* field.  
WNGGTO is the week number for the time model data in the GNSS time indicated by *GNSS-ID* corresponding to the tGGTO and given by the *weekNumber* field.  
A0GGTO is given by the *tA0* field.  
A1GGTO is given by the *tA1* field.  
A2GGTO is given by the *tA2* field.  
  
If the *tA1*and *tA2*are not included in the *GNSS-TimeModelElement*, the target device assumes A1GGTO and A2GGTO are equal to zero.

The GNSS system times in the IE *GNSS-TimeModelList* and used in the equation above are all given in Time of Week (TOW) and Week Number (WN) in the indicted GNSS specific system time. For conversion between TOW/WN and Day Number/Time of Day (*gnss-DayNumber*/*gnss-TimeOfDay*) a GNSS week consists of 7 days since the origin of the particular GNSS System time (with the week number count starting at 0), and a day consists of 86400 seconds.

#### – *GNSS-DifferentialCorrections*

The IE *GNSS-DifferentialCorrections* is used by the location server to provide differential GNSS corrections to the target device for a specific GNSS. Differential corrections can be provided for up to 3 signals per GNSS.

-- ASN1START

GNSS-DifferentialCorrections ::= SEQUENCE {

dgnss-RefTime INTEGER (0..3599),

dgnss-SgnTypeList DGNSS-SgnTypeList,

...

}

DGNSS-SgnTypeList ::= SEQUENCE (SIZE (1..3)) OF DGNSS-SgnTypeElement

DGNSS-SgnTypeElement ::= SEQUENCE {

gnss-SignalID GNSS-SignalID,

gnss-StatusHealth INTEGER (0..7),

dgnss-SatList DGNSS-SatList,

...

}

DGNSS-SatList ::= SEQUENCE (SIZE (1..64)) OF DGNSS-CorrectionsElement

DGNSS-CorrectionsElement ::= SEQUENCE {

svID SV-ID,

iod BIT STRING (SIZE(11)),

udre INTEGER (0..3),

pseudoRangeCor INTEGER (-2047..2047),

rangeRateCor INTEGER (-127..127),

udreGrowthRate INTEGER (0..7) OPTIONAL, -- Need ON

udreValidityTime INTEGER (0..7) OPTIONAL, -- Need ON

...

}

-- ASN1STOP

| *GNSS-DifferentialCorrections* field descriptions |
| --- |
| ***dgnss-RefTime***  This field specifies the time for which the DGNSS corrections are valid, modulo 1 hour. *dgnss-RefTime* is given in GNSS specific system time.  Scale factor 1‑second. |
| ***dgnss-SgnTypeList***  This list includes differential correction data for different GNSS signal types, identified by *GNSS-SignalID*. |
| ***gnss-StatusHealth***  This field specifies the status of the differential corrections. The values of this field and their respective meanings are defined as in table *gnss-StatusHealth* Value to Indication relation below.  The first six values in this field indicate valid differential corrections. When using the values described below, the "UDRE Scale Factor" value is applied to the UDRE values contained in the element. The purpose is to indicate an estimate in the amount of error in the corrections.  The value "110" indicates that the source of the differential corrections (e.g., reference station or external DGNSS network) is currently not being monitored. The value "111" indicates that the corrections provided by the source are invalid, as judged by the source. |
| ***dgnss-SatList***  This list includes differential correction data for different GNSS satellites, identified by *SV-ID*. |
| ***iod***  This field specifies the Issue of Data field which contains the identity for the *GNSS-NavigationModel.* |
| ***udre***  This field provides an estimate of the uncertainty (1-σ) in the corrections for the particular satellite. The value in this field shall be multiplied by the UDRE Scale Factor in the *gnss-StatusHealth* field to determine the final UDRE estimate for the particular satellite. The meanings of the values for this field are shown in the table *udre Value* to Indication relation below. |
| ***pseudoRangeCor***  This field specifies the correction to the pseudorange for the particular satellite at *dgnss-RefTime*, t0. The value of this field is given in metres and the scale factor is 0.32 metres in the range of ±655.04 metres. The method of calculating this field is described in [11].  If the location server has received a request for GNSS assistance data from a target device which included a request for the GNSS Navigation Model and DGNSS, the location server determines, for each satellite, if the navigation model stored by the target device is still suitable for use with DGNSS corrections and if so and if DGNSS corrections are supported the location server should send DGNSS corrections without including the GNSS Navigation Model.  The *iod* value sent for a satellite shall always be the IOD value that corresponds to the navigation model for which the pseudo-range corrections are applicable.  The target device shall only use the *pseudoRangeCor*value when the IOD value received matches its available navigation model.  Pseudo-range corrections are provided with respect to GNSS specific geodetic datum (e.g., PZ-90.02 if *GNSS‑ID* indicates GLONASS).  Scale factor 0.32 metres. |
| ***rangeRateCor***  This field specifies the rate-of-change of the pseudorange correction for the particular satellite, using the satellite ephemeris and clock corrections identified by the *iod* field. The value of this field is given in metres per second and the resolution is 0.032 metres/second in the range of ±4.064 metres/second. For some time t1 > t0, the corrections for *iod* are estimated by  PRC(t1,IOD) = PRC(t0, IOD) + RRC(t0,IOD)⋅(t1 - t0),  and the target device uses this to correct the pseudorange it measures at t1, PRm(t1,IOD), by  PR(t1, IOD) = PRm(t1, IOD) + PRC(t1, IOD) .  The location server always sends the RRC value that corresponds to the PRC value that it sends. The target device shall only use the RRC value when the *iod* value received matches its available navigation model.  Scale factor 0.032 metres/second. |
| ***udreGrowthRate***  This field provides an estimate of the growth rate of uncertainty (1-σ) in the corrections for the particular satellite identified by *SV-ID*. The estimated UDRE at time value specified in the *udreValidityTime**t1* is calculated as follows:  UDRE(*t0*+*t1*) = UDRE(*t0*) × *udreGrowthRate ,*  where *t0* is the DGNSS Reference Time *dgnss-RefTime*for which the corrections are valid, *t1* is the *udreValidityTime*  field, UDRE(*t0*) is the value of the *udre* field, and *udreGrowthRate* field is the factor as shown in the table Value of *udreGrowthRate* to Indication relation below. |
| ***udreValidityTime***  This field specifies the time when the *udreGrowthRate* field applies and is included if *udreGrowthRate* is included. The meaning of the values for this field is as shown in the table Value of *udreValidityTime* to Indication relation below. |

*gnss-StatusHealth* Value to Indication relation

|  |  |
| --- | --- |
| *gnss-StatusHealth Value* | Indication |
| 000 | UDRE Scale Factor = 1.0 |
| 001 | UDRE Scale Factor = 0.75 |
| 010 | UDRE Scale Factor = 0.5 |
| 011 | UDRE Scale Factor = 0.3 |
| 100 | UDRE Scale Factor = 0.2 |
| 101 | UDRE Scale Factor = 0.1 |
| 110 | Reference Station Transmission Not Monitored |
| 111 | Data is invalid - disregard |

*udre* Value to Indication relation

|  |  |
| --- | --- |
| *udre* Value | Indication |
| 00 | UDRE ≤ 1.0 m |
| 01 | 1.0 m < UDRE ≤ 4.0 m |
| 10 | 4.0 m < UDRE ≤ 8.0 m |
| 11 | 8.0 m < UDRE |

Value of *udreGrowthRate* to Indication relation

|  |  |
| --- | --- |
| **Value of *udreGrowthRate*** | **Indication** |
| 000 | 1.5 |
| 001 | 2 |
| 010 | 4 |
| 011 | 6 |
| 100 | 8 |
| 101 | 10 |
| 110 | 12 |
| 111 | 16 |

Value of *udreValidityTime* to Indication relation

|  |  |
| --- | --- |
| **Value of *udreValidityTime*** | **Indication**  **[seconds]** |
| 000 | 20 |
| 001 | 40 |
| 010 | 80 |
| 011 | 160 |
| 100 | 320 |
| 101 | 640 |
| 110 | 1280 |
| 111 | 2560 |

#### – *GNSS-NavigationModel*

The IE *GNSS-NavigationModel* is used by the location server to provide precise navigation data to the GNSS capable target device. In response to a request from a target device for GNSS Assistance Data, the location server determines whether to send the navigation model for a particular satellite to a target device based upon factors like the T-Toe limit specified by the target device and any request from the target device for DGNSS (see also *GNSS-DifferentialCorrections*). GNSS Orbit Model can be given in Keplerian parameters or as state vector in Earth-Centered Earth-Fixed coordinates, dependent on the *GNSS-ID* and the target device capabilities. The meaning of these parameters is defined in relevant ICDs of the particular GNSS and GNSS specific interpretations apply. For example, GPS and QZSS use the same model parameters but some parameters have a different interpretation [7].

-- ASN1START

GNSS-NavigationModel ::= SEQUENCE {

nonBroadcastIndFlag INTEGER (0..1),

gnss-SatelliteList GNSS-NavModelSatelliteList,

...

}

GNSS-NavModelSatelliteList ::= SEQUENCE (SIZE(1..64)) OF GNSS-NavModelSatelliteElement

GNSS-NavModelSatelliteElement ::= SEQUENCE {

svID SV-ID,

svHealth BIT STRING (SIZE(8)),

iod BIT STRING (SIZE(11)),

gnss-ClockModel GNSS-ClockModel,

gnss-OrbitModel GNSS-OrbitModel,

...,

[[ svHealthExt-v1240 BIT STRING (SIZE(4)) OPTIONAL -- Need ON

]]

}

GNSS-ClockModel ::= CHOICE {

standardClockModelList StandardClockModelList, -- Model-1

nav-ClockModel NAV-ClockModel, -- Model-2

cnav-ClockModel CNAV-ClockModel, -- Model-3

glonass-ClockModel GLONASS-ClockModel, -- Model-4

sbas-ClockModel SBAS-ClockModel, -- Model-5

...,

bds-ClockModel-r12 BDS-ClockModel-r12, -- Model-6

bds-ClockModel2-r16 BDS-ClockModel2-r16, -- Model-7

navic-ClockModel-r16 NavIC-ClockModel-r16 -- Model-8

}

GNSS-OrbitModel ::= CHOICE {

keplerianSet NavModelKeplerianSet, -- Model-1

nav-KeplerianSet NavModelNAV-KeplerianSet, -- Model-2

cnav-KeplerianSet NavModelCNAV-KeplerianSet, -- Model-3

glonass-ECEF NavModel-GLONASS-ECEF, -- Model-4

sbas-ECEF NavModel-SBAS-ECEF, -- Model-5

...,

bds-KeplerianSet-r12 NavModel-BDS-KeplerianSet-r12, -- Model-6

bds-KeplerianSet2-r16 NavModel-BDS-KeplerianSet2-r16, -- Model-7

navic-KeplerianSet-r16 NavModel-NavIC-KeplerianSet-r16 -- Model-8

}

-- ASN1STOP

| *GNSS-NavigationModel* field descriptions |
| --- |
| ***nonBroadcastIndFlag***  This field indicates if the *GNSS-NavigationModel* elements are not derived from satellite broadcast data or are given in a format not native to the GNSS. A value of 0 means the *GNSS-NavigationModel* data elements correspond to GNSS satellite broadcasted data; a value of 1 means the *GNSS-NavigationModel* data elements are not derived from satellite broadcast. |
| ***gnss-SatelliteList***  This list provides ephemeris and clock corrections for GNSS satellites indicated by *SV‑ID*. |
| ***svHealth***  This field specifies the satellite's current health. The health values are GNSS system specific. The interpretation of *svHealth* depends on the *GNSS‑ID* and is as shown in table GNSS to svHealth Bit String(8) relation below. |
| ***iod***  This field specifies the Issue of Data and contains the identity for GNSS Navigation Model.  In the case of broadcasted GPS NAV ephemeris, the *iod* contains the IODC as described in [4].  In the case of broadcasted Modernized GPS ephemeris, the *iod* contains the 11-bit parameter toe as defined in [4, Table 30-I] [6, Table 3.5-1].  In the case of broadcasted SBAS ephemeris, the *iod* contains the 8 bits Issue of Data as defined in [10] Message Type 9.  In the case of broadcasted QZSS QZS-L1 ephemeris, the *iod* contains the IODC as described in [7].  In the case of broadcasted QZSS QZS-L1C/L2C/L5 ephemeris, the *iod* contains the 11-bit parameter toe as defined in [7].  In the case of broadcasted GLONASS ephemeris, the *iod* contains the parameter tb as defined in [9].  In the case of broadcasted Galileo ephemeris, the *iod* contains the IOD index as described in [8].  In the case of broadcasted BDS B1I/B3I ephemeris, the *iod* contains 11 MSB bits of the toe as defined in [23], [50].  In the case of broadcasted BDS B1C/B2a ephemeris, the *iod* contains the IODC as described in [39], [49].  In the case of broadcasted NavIC ephemeris, the iod contains 11 MSB bits of the toe as defined in [38].  The interpretation of *iod* depends on the *GNSS‑ID* and is as shown in table GNSS to iod Bit String(11) relation below. |
| ***svHealthExt***  This field specifies the satellite's additional current health. The health values are GNSS system specific. The interpretation of *svHealthExt* depends on the *GNSS‑ID* and is as shown in table GNSS to svHealthExt Bit String(4) relation below. |

GNSS to svHealth Bit String(8) relation

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| GNSS | *svHealth* Bit String(8) | | | | | | | |
| Bit 1  (MSB) | Bit 2 | Bit 3 | Bit 4 | Bit 5 | Bit 6 | Bit 7 | Bit 8 (LSB) |
| GPS L1/CA(1) | SV Health [4] | | | | | | '0'  (reserved) | '0'  (reserved) |
| Modernized GPS(2) | L1C Health  [6] | L1 Health [4,5] | L2 Health  [4,5] | L5 Health [4,5] | '0'  (reserved) | '0'  (reserved) | '0'  (reserved) | '0'  (reserved) |
| SBAS(3) | Ranging  On (0),Off(1) [10] | Corrections On(0),Off(1) [10] | Integrity  On(0),Off(1)[10] | '0'  (reserved) | '0'  (reserved) | '0'  (reserved) | '0'  (reserved) | '0'  (reserved) |
| QZSS(4)  QZS-L1 | SV Health [7] | | | | | | '0'  (reserved) | '0'  (reserved) |
| QZSS(5)  QZS‑  L1C/L2C/L5 | L1C Health  [7] | L1 Health  [7] | L2 Health  [7] | L5 Health  [7] | '0'  (reserved) | '0'  (reserved) | '0'  (reserved) | '0'  (reserved) |
| GLONASS | Bn (MSB)  [9, page 30] | FT [9, Table 4.4] | | | | '0'  (reserved) | '0'  (reserved) | '0'  (reserved) |
| Galileo  [8, clause 5.1.9.3] | E5a Data Validity Status | E5b Data Validity Status | E1-B Data Validity Status | E5a Signal Health Status | | '0'  (reserved) | '0'  (reserved) | '0'  (reserved) |
| BDS(6) B1I  [23] | B1I Health (SatH1) [23], [50] | B3I Health (SatH1) [23], [50] | '0'  (reserved) | '0'  (reserved) | '0'  (reserved) | '0'  (reserved) | '0'  (reserved) | '0'  (reserved) |
| BDS(7) B1C  [39]/B2a [49] | Sat Clock Health [39], [49] | B1C Health  [39], [49] | B2a Health  [39],[49] | '0'  (reserved) | '0'  (reserved) | '0'  (reserved) | '0'  (reserved) | '0'  (reserved) |
| NavIC | L5 health | '0'  (reserved) | '0'  (reserved) | '0'  (reserved) | '0'  (reserved) | '0'  (reserved) | '0'  (reserved) | '0'  (reserved) |
| Note 1: If *GNSS‑ID* indicates 'gps', and GNSS Orbit Model-2 is included, this interpretation of *svHealth* applies.  Note 2: If *GNSS‑ID* indicates 'gps', and GNSS Orbit Model-3 is included, this interpretation of *svHealth* applies. If a certain signal is not supported on the satellite indicated by *SV‑ID*, the corresponding health bit shall be set to '1' (i.e., signal can not be used).  Note 3: *svHealth,* in the case that *GNSS‑ID* indicates 'sbas', includes the 5 LSBs of the Health included in GEO Almanac Message Parameters (Type 17) [10].  Note 4: If *GNSS‑ID* indicates 'qzss', and GNSS Orbit Model-2 is included, this interpretation of *svHealth* applies.  Note 5: If *GNSS‑ID* indicates 'qzss', and GNSS Orbit Model-3 is included, this interpretation of *svHealth* applies.  Note 6: If *GNSS‑ID* indicates 'bds', and GNSS Orbit Model-6 is included, this interpretation of *svHealth* applies.  Note 7: If *GNSS‑ID* indicates 'bds', and GNSS Orbit Model-7 is included, this interpretation of *svHealth* applies. | | | | | | | | |

GNSS to iod Bit String(11) relation

|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| GNSS | *iod* Bit String(11) | | | | | | | | | | |
| Bit 1  (MSB) | Bit 2 | Bit 3 | Bit 4 | Bit 5 | Bit 6 | Bit 7 | Bit 8 | Bit 9 | Bit 10 | Bit 11  (LSB) |
| GPS L1/CA | '0' | Issue of Data, Clock [4] | | | | | | | | | |
| Modernized GPS | toe (seconds, scale factor 300, range 0 – 604500) [4,5,6] | | | | | | | | | | |
| SBAS | '0' | '0' | '0' | Issue of Data ([10], Message Type 9) | | | | | | | |
| QZSS QZS-L1 | '0' | Issue of Data, Clock [7] | | | | | | | | | |
| QZSS  QZS-L1C/L2C/L5 | toe (seconds, scale factor 300, range 0 – 604500) [7] | | | | | | | | | | |
| GLONASS | '0' | '0' | '0' | '0' | tb (minutes, scale factor 15) [9] | | | | | | |
| Galileo I/NAV | '0' | IODnav [8] | | | | | | | | | |
| BDS B1I/B3I | 11 MSB bits of toe (seconds, scale factor 512, range 0 – 604672) [23], [50] | | | | | | | | | | |
| BDS B1C/B2a | '0' | Issue of Data, Clock [39], [49] | | | | | | | | | |
| NavIC | 11 MSB bits of toe (seconds, scale factor 512) [38] | | | | | | | | | | |

GNSS to svHealthExt Bit String(4) relation

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| GNSS | *svHealthExt* Bit String(4) | | | |
| Bit 1  (MSB) | Bit 2 | Bit 3 | Bit 4  (LSB) |
| Galileo [8, clause 5.1.9.3] | E5b Signal Health Status | | E1-B Signal Health Status | |

#### – *StandardClockModelList*

-- ASN1START

StandardClockModelList ::= SEQUENCE (SIZE(1..2)) OF StandardClockModelElement

StandardClockModelElement ::= SEQUENCE {

stanClockToc INTEGER (0..16383),

stanClockAF2 INTEGER (-32..31),

stanClockAF1 INTEGER (-1048576..1048575),

stanClockAF0 INTEGER (-1073741824..1073741823),

stanClockTgd INTEGER (-512..511) OPTIONAL, -- Need ON

sisa INTEGER (0..255),

stanModelID INTEGER (0..1) OPTIONAL, -- Need ON

...

}

-- ASN1STOP

| *StandardClockModelList* field descriptions |
| --- |
| ***standardClockModelList***  *gnss-ClockModel* Model-1 contains one or two clock model elements. If included, clock Model-1 shall be included once or twice depending on the target device capability.  If the target device is supporting multiple Galileo signals, the location server includes both F/Nav and I/Nav clock models in *gnss-ClockModel* if the location server assumes the target device to perform location information calculation using multiple signals. |
| ***stanClockToc***  Parameter toc defined in [8].  Scale factor 60 seconds. |
| ***stanClockAF2***  Parameter af2 defined in [8].  Scale factor 2-59 seconds/second2. |
| ***stanClockAF1***  Parameter af1 defined in [8].  Scale factor 2-46 seconds/second. |
| ***stanClockAF0***  Parameter af0 defined in [8].  Scale factor 2-34 seconds. |
| ***stanClockTgd***  Parameter TGD, Broadcast Group Delay (BGD), defined in [8].  Scale factor 2-32 seconds.  This field is required if the target device supports only single frequency Galileo signal. |
| ***sisa***  Signal-In-Space Accuracy (SISA), defined in [8] clause 5.1.11. |
| ***stanModelID***  This field specifies the identity of the clock model according to the table Value of *stanModelID* to Identity relation below. This field is required if the location server includes both F/Nav and I/Nav Galileo clock models in *gnss-ClockModel.* |

Value of *stanModelID* to Identity relation

|  |  |
| --- | --- |
| Value of *stanModelID* | Identity |
| 0 | I/Nav (E1,E5b) |
| 1 | F/Nav (E1,E5a) |

#### – *NAV-ClockModel*

-- ASN1START

NAV-ClockModel ::= SEQUENCE {

navToc INTEGER (0..37799),

navaf2 INTEGER (-128..127),

navaf1 INTEGER (-32768..32767),

navaf0 INTEGER (-2097152..2097151),

navTgd INTEGER (-128..127),

...

}

-- ASN1STOP

| *NAV-ClockModel* field descriptions |
| --- |
| ***navToc***  Parameter toc, time of clock (seconds) [4,7]  Scale factor 24 seconds. |
| ***navaf2***  Parameter af2, clock correction polynomial coefficient (sec/sec2) [4,7].  Scale factor 2-55 seconds/second2. |
| ***navaf1***  Parameter af1, clock correction polynomial coefficient (sec/sec) [4,7].  Scale factor 2-43 seconds/second. |
| ***navaf0***  Parameter af0, clock correction polynomial coefficient (seconds) [4,7].  Scale factor 2-31 seconds. |
| ***navTgd***  Parameter TGD, group delay (seconds) [4,7].  Scale factor 2-31 seconds. |

#### – *CNAV-ClockModel*

-- ASN1START

CNAV-ClockModel ::= SEQUENCE {

cnavToc INTEGER (0..2015),

cnavTop INTEGER (0..2015),

cnavURA0 INTEGER (-16..15),

cnavURA1 INTEGER (0..7),

cnavURA2 INTEGER (0..7),

cnavAf2 INTEGER (-512..511),

cnavAf1 INTEGER (-524288..524287),

cnavAf0 INTEGER (-33554432..33554431),

cnavTgd INTEGER (-4096..4095),

cnavISCl1cp INTEGER (-4096..4095) OPTIONAL, -- Need ON

cnavISCl1cd INTEGER (-4096..4095) OPTIONAL, -- Need ON

cnavISCl1ca INTEGER (-4096..4095) OPTIONAL, -- Need ON

cnavISCl2c INTEGER (-4096..4095) OPTIONAL, -- Need ON

cnavISCl5i5 INTEGER (-4096..4095) OPTIONAL, -- Need ON

cnavISCl5q5 INTEGER (-4096..4095) OPTIONAL, -- Need ON

...

}

-- ASN1STOP

| *CNAV-ClockModel* field descriptions |
| --- |
| ***cnavToc***  Parameter toc, clock data reference time of week (seconds) [4,5,6,7].  Scale factor 300 seconds. |
| ***cnavTop***  Parameter top, clock data predict time of week (seconds) [4,5,6,7].  Scale factor 300 seconds |
| ***cnavURA0***  Parameter URAoc Index, SV clock accuracy index (dimensionless) [4,5,6,7]. |
| ***cnavURA1***  Parameter URAoc1 Index, SV clock accuracy change index (dimensionless) [4,5,6,7]. |
| ***cnavURA2***  Parameter URAoc2 Index, SV clock accuracy change rate index (dimensionless) [4,5,6,7]. |
| ***cnavAf2***  Parameter af2-n, SV clock drift rate correction coefficient (sec/sec2) [4,5,6,7].  Scale factor 2-60 seconds/second2. |
| ***cnavAf1***  Parameter af1-n, SV clock drift correction coefficient (sec/sec) [4,5,6,7].  Scale factor 2-48 seconds/second. |
| ***cnavAf0***  Parameter af0-n, SV clock bias correction coefficient (seconds) [4,5,6,7].  Scale factor 2-35 seconds. |
| ***cnavTgd***  Parameter TGD, Group delay correction (seconds) [4,5,6,7].  Scale factor 2-35 seconds. |
| ***cnavISCl1cp***  Parameter ISCL1CP, inter signal group delay correction (seconds) [6,7].  Scale factor 2-35 seconds.  The location server should include this field if the target device is GPS capable and supports the L1C signal. |
| ***cnavISCl1cd***  Parameter ISCL1CD, inter signal group delay correction (seconds) [6,7].  Scale factor 2-35 seconds.  The location server should include this field if the target device is GPS capable and supports the L1C signal. |
| ***cnavISCl1ca***  Parameter ISCL1C/A, inter signal group delay correction (seconds) [4,5,7].  Scale factor 2-35 seconds.  The location server should include this field if the target device is GPS capable and supports the L1CA signal. |
| ***cnavISCl2c***  Parameter ISCL2C, inter signal group delay correction (seconds) [4,5,7].  Scale factor 2-35 seconds.  The location server should include this field if the target device is GPS capable and supports the L2C signal. |
| ***cnavISCl5i5***  Parameter ISCL5I5, inter signal group delay correction (seconds) [5,7].  Scale factor 2-35 seconds.  The location server should include this field if the target device is GPS capable and supports the L5 signal. |
| ***cnavISCl5q5***  Parameter ISCL5Q5, inter signal group delay correction (seconds) [5,7].  Scale factor 2-35 seconds.  The location server should include this field if the target device is GPS capable and supports the L5 signal. |

#### – *GLONASS-ClockModel*

-- ASN1START

GLONASS-ClockModel ::= SEQUENCE {

gloTau INTEGER (-2097152..2097151),

gloGamma INTEGER (-1024..1023),

gloDeltaTau INTEGER (-16..15) OPTIONAL, -- Need ON

...

}

-- ASN1STOP

| *GLONASS-ClockModel* field descriptions |
| --- |
| ***gloTau***  Parameter n(tb), satellite clock offset (seconds) [9].  Scale factor 2-30 seconds. |
| ***gloGamma***  Parameter n(tb), relative frequency offset from nominal value (dimensionless) [9].  Scale factor 2-40. |
| ***gloDeltaTau***  Parameter n, time difference between transmission in G2 and G1 (seconds) [9].  Scale factor 2-30 seconds.  The location server should include this parameter if the target device is dual frequency GLONASS receiver capable. |

#### – *SBAS-ClockModel*

-- ASN1START

SBAS-ClockModel ::= SEQUENCE {

sbasTo INTEGER (0..5399),

sbasAgfo INTEGER (-2048..2047),

sbasAgf1 INTEGER (-128..127),

...

}

-- ASN1STOP

| *SBAS-ClockModel* field descriptions |
| --- |
| ***sbasTo***  Parameter t0 [10].  Scale factor 16 seconds. |
| ***sbasAgfo***  Parameter aGfo [10].  Scale factor 2-31 seconds. |
| ***sbasAgf1***  Parameter aGf1 [10].  Scale factor 2-40 seconds/second. |

#### – *BDS-ClockModel*

The IE *BDS-ClockModel* is used for BDS B1I defined in [23] and BDS B3I defined in [50].

-- ASN1START

BDS-ClockModel-r12 ::= SEQUENCE {

bdsAODC-r12 INTEGER (0..31),

bdsToc-r12 INTEGER (0..131071),

bdsA0-r12 INTEGER (-8388608..8388607),

bdsA1-r12 INTEGER (-2097152..2097151),

bdsA2-r12 INTEGER (-1024..1023),

bdsTgd1-r12 INTEGER (-512..511),

...,

[[ bdsTgd2-r16 INTEGER (-512..511) OPTIONAL -- Need ON

]]

}

-- ASN1STOP

| *BDS-ClockModel* field descriptions |
| --- |
| ***bdsAODC***  Parameter Age of Data, Clock (AODC), see [23], [50], Table 5-6. |
| ***bdsToc***  Parameter Toc, Time of clock (seconds) [23], [50].  Scale factor 23 seconds. |
| ***bdsA0***  Parameter a0, Clock correction polynomial coefficient (seconds) [23], [50].  Scale factor 2-33 seconds. |
| ***bdsA1***  Parameter a1, Clock correction polynomial coefficient (sec/sec) [23], [50].  Scale factor 2-50 sec/sec. |
| ***bdsA2***  Parameter a2, Clock correction polynomial coefficient (sec/sec2) [23], [50].  Scale factor 2-66 sec/sec2. |
| ***bdsTgd1***  Parameter Equipment group delay differential TGD1 [23], [50].  Scale factor is 0.1 nanosecond. |
| ***bdsTgd2***  Parameter Equipment group delay differential TGD2 [23], [50].  Scale factor is 0.1 nanosecond. |

#### – *BDS-ClockModel2*

The IE *BDS-ClockModel2* is used for BDS B1C defined in [39] and BDS B2a defined in [49].

-- ASN1START

BDS-ClockModel2-r16 ::= SEQUENCE {

bdsToc-r16 INTEGER (0..2047),

bdsA0-r16 INTEGER (-16777216..16777215),

bdsA1-r16 INTEGER (-2097152..2097151),

bdsA2-r16 INTEGER (-1024..1023),

bdsTgdB1Cp-r16 INTEGER (-2048..2047),

bdsIscB1Cd-r16 INTEGER (-2048..2047),

...,

[[ bdsTgdB2ap-r17 INTEGER (-2048..2047) OPTIONAL, -- Need ON

bdsIscB2ad-r17 INTEGER (-2048..2047) OPTIONAL -- Need ON

]]

}

-- ASN1STOP

| *BDS-ClockModel2* field descriptions |
| --- |
| ***bdsToc***  Parameter Toc, Clock correction parameters reference time (seconds), see [39], 7.5.1 and [49], 7.5.1.  Scale factor 300 seconds. |
| ***bdsA0***  Parameter a0, Satellite clock time bias correction coefficient (seconds), see [39], 7.5.1 and [49], 7.5.1.  Scale factor 2-34 seconds. |
| ***bdsA1***  Parameter a1, Satellite clock time drift correction coefficient (sec/sec), see [39], 7.5.1 and [49], 7.5.1.  Scale factor 2-50 sec/sec. |
| ***bdsA2***  Parameter a2, Satellite clock time drift rate correction coefficient (sec/sec2), see [39], 7.5.1 and [49], 7.5.1.  Scale factor 2-66 sec/sec2. |
| ***bdsTgdB1Cp***  Parameter TGDB1Cp Group delay differential of the B1C pilot component (seconds), see [39], 7.6.1 and [49], 7.6.1.  Scale factor is 2-34 seconds. |
| ***bdsIscB1Cd***  Parameter ISCB1Cd Group delay differential between the B1C data and pilot components (seconds), see [39], 7.6.1.  Scale factor is 2-34 seconds. |
| ***bdsTgdB2ap***  Parameter TGDB2ap Group delay differential of the B2a pilot component (seconds), see [39], 7.6.1 and [49], 7.6.1.  Scale factor is 2-34 seconds. |
| ***bdsIscB2ad***  Parameter ISCB2ad Group delay differential between the B2a data and pilot components (seconds), see [49], 7.6.1.  Scale factor is 2-34 seconds. |

#### – *NavIC-ClockModel*

-- ASN1START

NavIC-ClockModel-r16 ::= SEQUENCE {

navic-Toc-r16 INTEGER (0..65535),

navic-af2-r16 INTEGER (-128..127),

navic-af1-r16 INTEGER (-32768..32767),

navic-af0-r16 INTEGER (-2097152..2097151),

navic-Tgd-r16 INTEGER (-128..127),

...

}

-- ASN1STOP

| *NavIC-ClockModel* field descriptions |
| --- |
| ***navic-Toc***  Parameter toc, time of clock (seconds) [38], Table-11.  Scale factor 24 seconds. |
| ***navic-af2***  Parameter af2, clock correction polynomial coefficient (sec/sec2) [38].  Scale factor 2-55 seconds/second2. |
| ***navic-af1***  Parameter af1, clock correction polynomial coefficient (sec/sec) [38].  Scale factor 2-43 seconds/second. |
| ***navic-af0***  Parameter af0, clock correction polynomial coefficient (seconds) [38].  Scale factor 2-31 seconds. |
| ***navic-Tgd***  Parameter TGD, group delay (seconds) [38].  Scale factor 2-31 seconds. |

#### – *NavModelKeplerianSet*

-- ASN1START

NavModelKeplerianSet ::= SEQUENCE {

keplerToe INTEGER (0 .. 16383),

keplerW INTEGER (-2147483648..2147483647),

keplerDeltaN INTEGER (-32768..32767),

keplerM0 INTEGER (-2147483648..2147483647),

keplerOmegaDot INTEGER (-8388608.. 8388607),

keplerE INTEGER (0..4294967295),

keplerIDot INTEGER (-8192..8191),

keplerAPowerHalf INTEGER (0.. 4294967295),

keplerI0 INTEGER (-2147483648..2147483647),

keplerOmega0 INTEGER (-2147483648..2147483647),

keplerCrs INTEGER (-32768..32767),

keplerCis INTEGER (-32768..32767),

keplerCus INTEGER (-32768..32767),

keplerCrc INTEGER (-32768..32767),

keplerCic INTEGER (-32768..32767),

keplerCuc INTEGER (-32768..32767),

...

}

-- ASN1STOP

| *NavModelKeplerianSet* field descriptions |
| --- |
| ***keplerToe***  Parameter toe, time-of-ephemeris in seconds [8].  Scale factor 60 seconds. |
| ***keplerW***  Parameter ω, argument of perigee (semi-circles) [8].  Scale factor 2-31 semi-circles. |
| ***keplerDeltaN***  Parameter n, mean motion difference from computed value (semi-circles/sec) [8].  Scale factor 2-43 semi-circles/second. |
| ***keplerM0***  Parameter M0, mean anomaly at reference time (semi-circles) [8].  Scale factor 2-31 semi-circles. |
| ***keplerOmegaDot***  Parameter OMEGAdot, rate of change of right ascension (semi-circles/sec) [8].  Scale factor 2-43 semi-circles/second. |
| ***keplerE***  Parameter e, eccentricity [8].  Scale factor 2-33. |
| ***KeplerIDot***  Parameter Idot, rate of change of inclination angle (semi-circles/sec) [8].  Scale factor 2-43 semi-circles/second. |
| ***keplerAPowerHalf***  Parameter sqrtA, square root of semi-major Axis in (metres) ½ [8].  Scale factor 2-19 metres½. |
| ***keplerI0***  Parameter i0, inclination angle at reference time (semi-circles) [8].  Scale factor 2-31 semi-circles. |
| ***keplerOmega0***  Parameter OMEGA0, longitude of ascending node of orbit plane at weekly epoch (semi-circles) [8].  Scale factor 2-31 semi-circles. |
| ***keplerCrs***  Parameter Crs, amplitude of the sine harmonic correction term to the orbit radius (metres) [8].  Scale factor 2-5 metres. |
| ***keplerCis***  Parameter Cis, amplitude of the sine harmonic correction term to the angle of inclination (radians) [8].  Scale factor 2-29 radians. |
| ***keplerCus***  Parameter Cus, amplitude of the sine harmonic correction term to the argument of latitude (radians) [8].  Scale factor 2-29 radians. |
| ***keplerCrc***  Parameter Crc, amplitude of the cosine harmonic correction term to the orbit radius (metres) [8].  Scale factor 2-5 metres. |
| ***keplerCic***  Parameter Cic, amplitude of the cosine harmonic correction term to the angle of inclination (radians) [8].  Scale factor 2-29 radians. |
| ***keplerCuc***  Parameter Cuc, amplitude of the cosine harmonic correction term to the argument of latitude (radians) [8].  Scale factor 2-29 radians. |

#### – *NavModelNAV-KeplerianSet*

-- ASN1START

NavModelNAV-KeplerianSet ::= SEQUENCE {

navURA INTEGER (0..15),

navFitFlag INTEGER (0..1),

navToe INTEGER (0..37799),

navOmega INTEGER (-2147483648..2147483647),

navDeltaN INTEGER (-32768..32767),

navM0 INTEGER (-2147483648..2147483647),

navOmegaADot INTEGER (-8388608..8388607),

navE INTEGER (0..4294967295),

navIDot INTEGER (-8192..8191),

navAPowerHalf INTEGER (0..4294967295),

navI0 INTEGER (-2147483648..2147483647),

navOmegaA0 INTEGER (-2147483648..2147483647),

navCrs INTEGER (-32768..32767),

navCis INTEGER (-32768..32767),

navCus INTEGER (-32768..32767),

navCrc INTEGER (-32768..32767),

navCic INTEGER (-32768..32767),

navCuc INTEGER (-32768..32767),

addNAVparam SEQUENCE {

ephemCodeOnL2 INTEGER (0..3),

ephemL2Pflag INTEGER (0..1),

ephemSF1Rsvd SEQUENCE {

reserved1 INTEGER (0..8388607), -- 23-bit field

reserved2 INTEGER (0..16777215), -- 24-bit field

reserved3 INTEGER (0..16777215), -- 24-bit field

reserved4 INTEGER (0..65535) -- 16-bit field

},

ephemAODA INTEGER (0..31)

} OPTIONAL, -- Need ON

...

}

-- ASN1STOP

| *NavModelNAV-KeplerianSet* field descriptions |
| --- |
| ***navURA***  Parameter URA Index, SV accuracy (dimensionless) [4,7]. |
| ***navFitFlag***  Parameter Fit Interval Flag, fit interval indication (dimensionless) [4,7] |
| ***navToe***  Parameter toe, time of ephemeris (seconds) [4,7].  Scale factor 24 seconds. |
| ***navOmega***  Parameter ω, argument of perigee (semi-circles) [4,7].  Scale factor 2-31 semi-circles. |
| ***navDeltaN***  Parameter Δn, mean motion difference from computed value (semi-circles/sec) [4,7].  Scale factor 2-43 semi-circles/second. |
| ***navM0***  Parameter M0, mean anomaly at reference time (semi-circles) [4,7].  Scale factor 2-31 semi-circles. |
| ***navOmegaADot***  Parameter , rate of right ascension (semi-circles/sec) [4,7].  Scale factor 2-43 semi-circles/second. |
| ***navE***  Parameter e, eccentricity (dimensionless) [4,7].  Scale factor 2-33. |
| ***navIDot***  Parameter IDOT, rate of inclination angle (semi-circles/sec) [4,7].  Scale factor 2-43 semi-circles/second. |
| ***navAPowerHalf***  Parameter , square root of semi-major axis (metres/2) [4,7].  Scale factor 2-19 metres½. |
| ***navI0***  Parameter i0, inclination angle at reference time (semi-circles) [4,7].  Scale factor 2-31 semi-circles. |
| ***navOmegaA0***  Parameter 0, longitude of ascending node of orbit plane at weekly epoch (semi-circles) [4,7].  Scale factor 2-31 semi-circles. |
| ***navCrs***  Parameter Crs, amplitude of sine harmonic correction term to the orbit radius (metres) [4,7].  Scale factor 2-5 metres. |
| ***navCis***  Parameter Cis, amplitude of sine harmonic correction term to the angle of inclination (radians) [4,7].  Scale factor 2-29 radians. |
| ***navCus***  Parameter Cus, amplitude of sine harmonic correction term to the argument of latitude (radians) [4,7].  Scale factor 2-29 radians. |
| ***navCrc***  Parameter Crc, amplitude of cosine harmonic correction term to the orbit radius (metres) [4,7].  Scale factor 2-5 metres. |
| ***navCic***  Parameter Cic, amplitude of cosine harmonic correction term to the angle of inclination (radians) [4,7].  Scale factor 2-29 radians. |
| ***navCuc***  Parameter Cuc, amplitude of cosine harmonic correction term to the argument of latitude (radians) [4,7].  Scale factor 2-29 radians. |
| ***addNAVparam***  These fields include data and reserved bits in the GPS NAV message [4,14].  These additional navigation parameters, if provided by the location server, allow the target device to perform data wipe-off similar to what is done by the target device with the *GNSS-DataBitAssistance.* |

#### – *NavModelCNAV-KeplerianSet*

-- ASN1START

NavModelCNAV-KeplerianSet ::= SEQUENCE {

cnavTop INTEGER (0..2015),

cnavURAindex INTEGER (-16..15),

cnavDeltaA INTEGER (-33554432..33554431),

cnavAdot INTEGER (-16777216..16777215),

cnavDeltaNo INTEGER (-65536..65535),

cnavDeltaNoDot INTEGER (-4194304..4194303),

cnavMo INTEGER (-4294967296..4294967295),

cnavE INTEGER (0..8589934591),

cnavOmega INTEGER (-4294967296..4294967295),

cnavOMEGA0 INTEGER (-4294967296..4294967295),

cnavDeltaOmegaDot INTEGER (-65536..65535),

cnavIo INTEGER (-4294967296..4294967295),

cnavIoDot INTEGER (-16384..16383),

cnavCis INTEGER (-32768..32767),

cnavCic INTEGER (-32768..32767),

cnavCrs INTEGER (-8388608..8388607),

cnavCrc INTEGER (-8388608..8388607),

cnavCus INTEGER (-1048576..1048575),

cnavCuc INTEGER (-1048576..1048575),

...

}

-- ASN1STOP

| *NavModelCNAV-KeplerianSet* field descriptions |
| --- |
| ***cnavTop***  Parameter top, data predict time of week (seconds) [4,5,6,7].  Scale factor 300 seconds. |
| ***cnavURAindex***  Parameter URAoe Index, SV accuracy (dimensionless) [4,5,6,7]. |
| ***cnavDeltaA***  Parameter A, semi-major axis difference at reference time (metres) [4,5,6,7].  Scale factor 2-9 metres. |
| ***cnavAdot***  Parameter , change rate in semi-major axis (metres/second) [4,5,6,7].  Scale factor 2-21 metres/second. |
| ***cnavDeltaNo***  Parameter n0, mean motion difference from computed value at reference time (semi-circles/sec) [4,5,6,7].  Scale factor 2-44 semi-circles/second. |
| ***cnavDeltaNoDot***  Parameter , rate of mean motion difference from computed value (semi-circles/sec2) [4,5,6,7].  Scale factor 2-57 semi-circles/second2. |
| ***cnavMo***  Parameter M0-n, mean anomaly at reference time (semi-circles) [4,5,6,7].  Scale factor 2-32 semi-circles. |
| ***cnavE***  Parameter en, eccentricity (dimensionless) [4,5,6,7].  Scale factor 2-34. |
| ***cnavOmega***  Parameter n, argument of perigee (semi-circles) [4,5,6,7].  Scale factor 2-32 semi-circles. |
| ***cnavOMEGA0***  Parameter 0-n, reference right ascension angle (semi-circles) [4,5,6,7].  Scale factor 2-32 semi-circles. |
| ***cnavDeltaOmegaDot***  Parameter , rate of right ascension difference (semi-circles/sec) [4,5,6,7].  Scale factor 2-44 semi-circles/second. |
| ***cnavIo***  Parameter io-n, inclination angle at reference time (semi-circles) [4,5,6,7].  Scale factor 2-32 semi-circles. |
| ***cnavIoDot***  Parameter I0-n-DOT, rate of inclination angle (semi-circles/sec) [4,5,6,7].  Scale factor 2-44 semi-circles/second. |
| ***cnavCis***  Parameter Cis-n, amplitude of sine harmonic correction term to the angle of inclination (radians) [4,5,6,7].  Scale factor 2-30 radians. |
| ***cnavCic***  Parameter Cic-n, amplitude of cosine harmonic correction term to the angle of inclination (radians) [4,5,6,7].  Scale factor 2-30 radians. |
| ***cnavCrs***  Parameter Crs-n, amplitude of sine harmonic correction term to the orbit radius (metres) [4,5,6,7].  Scale factor 2-8 metres. |
| ***cnavCrc***  Parameter Crc-n, amplitude of cosine harmonic correction term to the orbit radius (metres) [4,5,6,7].  Scale factor 2-8 metres. |
| ***cnavCus***  Parameter Cus-n, amplitude of the sine harmonic correction term to the argument of latitude (radians) [4,5,6,7].  Scale factor 2-30 radians. |
| ***cnavCuc***  Parameter Cuc-n, amplitude of cosine harmonic correction term to the argument of latitude (radians) [4,5,6,7].  Scale factor 2-30 radians. |

#### – *NavModel-GLONASS-ECEF*

-- ASN1START

NavModel-GLONASS-ECEF ::= SEQUENCE {

gloEn INTEGER (0..31),

gloP1 BIT STRING (SIZE(2)),

gloP2 BOOLEAN,

gloM INTEGER (0..3),

gloX INTEGER (-67108864..67108863),

gloXdot INTEGER (-8388608..8388607),

gloXdotdot INTEGER (-16..15),

gloY INTEGER (-67108864..67108863),

gloYdot INTEGER (-8388608..8388607),

gloYdotdot INTEGER (-16..15),

gloZ INTEGER (-67108864..67108863),

gloZdot INTEGER (-8388608..8388607),

gloZdotdot INTEGER (-16..15),

...

}

-- ASN1STOP

| *NavModel-GLONASS-ECEF* field descriptions |
| --- |
| ***gloEn***  Parameter En, age of data (days) [9].  Scale factor 1 days. |
| ***gloP1***  Parameter P1, time interval between two adjacent values of tb (minutes) [9]. |
| ***gloP2***  Parameter P2, change of tb flag (dimensionless) [9]. |
| ***gloM***  Parameter M, type of satellite (dimensionless) [9]. |
| ***gloX***  Parameter , x-coordinate of satellite at time tb (kilometres) [9].  Scale factor 2-11 kilometres. |
| ***gloXdot***  Parameter , x-coordinate of satellite velocity at time tb (kilometres/second) [9].  Scale factor 2-20 kilometres/second. |
| ***gloXdotdot***  Parameter , x-coordinate of satellite acceleration at time tb (kilometres/second2) [9].  Scale factor 2-30 kilometres/second2. |
| ***gloY***  Parameter , y-coordinate of satellite at time tb (kilometres) [9].  Scale factor 2-11 kilometres. |
| ***gloYdot***  Parameter , y-coordinate of satellite velocity at time tb (kilometres/second) [9].  Scale factor 2-20 kilometres/second. |
| ***gloYdotdot***  Parameter , y-coordinate of satellite acceleration at time tb (kilometres/second2) [9].  Scale factor 2-30 kilometres/second2. |
| ***gloZ***  Parameter , z-coordinate of satellite at time tb (kilometres) [9].  Scale factor 2-11 kilometres. |
| ***gloZdot***  Parameter , z-coordinate of satellite velocity at time tb (kilometres/second) [9].  Scale factor 2-20 kilometres/second. |
| ***gloZdotdot***  Parameter , z-coordinate of satellite acceleration at time tb (kilometres/second2) [9].  Scale factor 2-30 kilometres/second2. |

#### – *NavModel-SBAS-ECEF*

-- ASN1START

NavModel-SBAS-ECEF ::= SEQUENCE {

sbasTo INTEGER (0..5399) OPTIONAL, -- Cond ClockModel

sbasAccuracy BIT STRING (SIZE(4)),

sbasXg INTEGER (-536870912..536870911),

sbasYg INTEGER (-536870912..536870911),

sbasZg INTEGER (-16777216..16777215),

sbasXgDot INTEGER (-65536..65535),

sbasYgDot INTEGER (-65536..65535),

sbasZgDot INTEGER (-131072..131071),

sbasXgDotDot INTEGER (-512..511),

sbagYgDotDot INTEGER (-512..511),

sbasZgDotDot INTEGER (-512..511),

...

}

-- ASN1STOP

| Conditional presence | Explanation |
| --- | --- |
| *ClockModel* | This field is mandatory present if *gnss-ClockModel* Model‑5 is not included; otherwise it is not present. |

| *NavModel-SBAS-ECEF* field descriptions |
| --- |
| ***sbasTo***  Parameter t0, time of applicability (seconds) [10].  Scale factor 16 seconds. |
| ***sbasAccuracy***  Parameter Accuracy, (dimensionless) [10]. |
| ***sbasXg***  Parameter XG, (metres) [10].  Scale factor 0.08 metres. |
| ***sbasYg***  Parameter YG, (metres) [10].  Scale factor 0.08 metres. |
| ***sbasZg***  Parameter ZG, (metres) [10].  Scale factor 0.4 metres. |
| ***sbasXgDot***  Parameter XG, Rate‑of‑Change, (metres/second) [10].  Scale factor 0.000625 metres/second. |
| ***sbasYgDot***  Parameter YG, Rate‑of‑Change, (metres/second) [10]  Scale factor 0.000625 metres/second. |
| ***sbasZgDot***  Parameter ZG, Rate‑of‑Change, (metres/second) [10].  Scale factor 0.004 metres/second. |
| ***sbasXgDotDot***  Parameter XG,Acceleration, (metres/second2) [10].  Scale factor 0.0000125 metres/second2. |
| ***sbagYgDotDot***  Parameter YG, Acceleration, (metres/second2) [10].  Scale factor 0.0000125 metres/second2. |
| ***sbasZgDotDot***  Parameter ZG Acceleration, (metres/second2) [10].  Scale factor 0.0000625 metres/second2. |

#### – *NavModel-BDS-KeplerianSet*

The IE *NavModel-BDS-KeplerianSet* is used for BDS B1I defined in [23], [50].

-- ASN1START

NavModel-BDS-KeplerianSet-r12 ::= SEQUENCE {

bdsAODE-r12 INTEGER (0..31),

bdsURAI-r12 INTEGER (0..15),

bdsToe-r12 INTEGER (0..131071),

bdsAPowerHalf-r12 INTEGER (0..4294967295),

bdsE-r12 INTEGER (0..4294967295),

bdsW-r12 INTEGER (-2147483648..2147483647),

bdsDeltaN-r12 INTEGER (-32768..32767),

bdsM0-r12 INTEGER (-2147483648..2147483647),

bdsOmega0-r12 INTEGER (-2147483648..2147483647),

bdsOmegaDot-r12 INTEGER (-8388608..8388607),

bdsI0-r12 INTEGER (-2147483648..2147483647),

bdsIDot-r12 INTEGER (-8192..8191),

bdsCuc-r12 INTEGER (-131072..131071),

bdsCus-r12 INTEGER (-131072..131071),

bdsCrc-r12 INTEGER (-131072..131071),

bdsCrs-r12 INTEGER (-131072..131071),

bdsCic-r12 INTEGER (-131072..131071),

bdsCis-r12 INTEGER (-131072..131071),

...

}

-- ASN1STOP

| *NavModel-BDS-KeplerianSet* field descriptions |
| --- |
| ***bdsAODE***  Parameter Age of Data, Ephemeris (AODE), see [23], [50], Table 5-8. |
| ***bdsURAI***  Parameter URA Index, URA is used to describe the signal-in-space accuracy in metres as defined in [23], [50]. |
| ***bdsToe***  Parameter toe, Ephemeris reference time (seconds) [23], [50].  Scale factor 23 seconds. |
| ***bdsAPowerHalf***  Parameter A1/2, Square root of semi-major axis (metres/2) [23], [50].  Scale factor 2-19 metres/2. |
| ***bdsE***  Parameter e, Eccentricity, dimensionless [23], [50].  Scale factor 2-33. |
| ***bdsW***  Parameter , Argument of perigee (semi-circles) [23], [50].  Scale factor 2-31 semi-circles. |
| ***bdsDeltaN***  Parameter n, Mean motion difference from computed value (semi-circles/sec) [23], [50].  Scale factor 2-43 semi-circles/second. |
| ***bdsM0***  Parameter M0, Mean anomaly at reference time (semi-circles) [23], [50].  Scale factor 2-31 semi-circles. |
| ***bdsOmega0***  Parameter 0, Longitude of ascending node of orbital of plane computed according to reference time (semi-circles) [23], [50].  Scale factor 2-31 semi-circles. |
| ***bdsOmegaDot***  Parameter  Rate of right ascension (semi-circles/sec) [23], [50].  Scale factor 2-43 semi-circles/second. |
| ***bdsI0***  Parameter i0, Inclination angle at reference time (semi-circles) [23], [50].  Scale factor 2-31 semi-circles. |
| ***bdsIDot***  Parameter Idot, Rate of inclination angle (semi-circles/sec) [23], [50].  Scale factor 2-43 semi-circles/second. |
| ***bdsCuc***  Parameter Cuc, Amplitude of cosine harmonic correction term to the argument of latitude (radians) [23], [50].  Scale factor 2-31 radians. |
| ***bdsCus***  Parameter Cus, Amplitude of sine harmonic correction term to the argument of latitude (radians) [23], [50].  Scale factor 2-31 radians. |
| ***bdsCrc***  Parameter Crc, Amplitude of cosine harmonic correction term to the orbit radius (metres) [23], [50].  Scale factor 2-6 metres. |
| ***bdsCrs***  Parameter Crs, Amplitude of sine harmonic correction term to the orbit radius (metres) [23], [50].  Scale factor 2-6 metres. |
| ***bdsCic***  Parameter Cic, Amplitude of cosine harmonic correction term to the angle of inclination (radians) [23], [50].  Scale factor 2-31 radians. |
| ***bdsCis***  Parameter Cis, Amplitude of sine harmonic correction term to the angle of inclination (radians) [23], [50].  Scale factor 2-31 radians. |

#### – *NavModel-BDS-KeplerianSet2*

The IE *NavModel-BDS-KeplerianSet2* is used for BDS B1C and BDS B2a defined in [39], [49].

-- ASN1START

NavModel-BDS-KeplerianSet2-r16 ::= SEQUENCE {

bdsIODE-r16 INTEGER (0..255),

bdsToe-r16 INTEGER (0..2047),

bdsDeltaA-r16 INTEGER (-33554432..33554431),

bdsAdot-r16 INTEGER (-16777216..16777216),

bdsDeltaN0-r16 INTEGER (-65536..65535),

bdsDeltaN0dot-r16 INTEGER (-4194304..4194303),

bdsM0-r16 INTEGER (-4294967296..4294967295),

bdsE-r16 INTEGER (0..8589934591),

bdsOmega-r16 INTEGER (-4294967296..4294967295),

bdsOmega0-r16 INTEGER (-4294967296..4294967295),

bdsI0-r16 INTEGER (-4294967296..4294967295),

bdsOmegaDot-r16 INTEGER (-262144..262143),

bdsI0Dot-r16 INTEGER (-16384..16383),

bdsCuc-r16 INTEGER (-1048576..1048575),

bdsCus-r16 INTEGER (-1048576..1048575),

bdsCrc-r16 INTEGER (-8388608..8388607),

bdsCrs-r16 INTEGER (-8388608..8388607),

bdsCic-r16 INTEGER (-32768..32767),

bdsCis-r16 INTEGER (-32768..32767),

...

}

-- ASN1STOP

| *NavModel-BDS-KeplerianSet2* field descriptions |
| --- |
| ***bdsIODE***  Parameter, Issue Of Data, Ephemeris (IODE), see [39], 7.4.1 and [49], 7.4.1. |
| ***bdsToe***  Parameter toe, Ephemeris reference time (seconds), defined in [39], 7.7.1 and [49], 7.7.1.  Scale factor 300 seconds. |
| ***bdsDeltaA***  Parameter A, Semi-major axis difference at reference time (metre), defined in [39], 7.7.1 and [49], 7.7.1.  Scale factor 2-9 metres. |
| ***bdsAdot***  Parameter , Change rate in semi-major axis (metre/second), defined in [39], 7.7.1 and [49], 7.7.1.  Scale factor 2-21 metre/second.  The value 16777216 is not signalled. |
| ***bdsDeltaN0***  Parameter n0, Mean motion difference from computed value at reference time (semi-circles /sec), defined in [39], 7.7.1 and [49], 7.7.1.  Scale factor 2-44 semi-circles /second. |
| ***bdsDeltaN0dot***  Parameter n0dot, Rate of mean motion difference from computed value at reference time (semi-circles /sec2), defined in [39], 7.7.1 and [49], 7.7.1.  Scale factor 2-57 semi-circles /second2. |
| ***bdsM0***  Parameter M0, Mean anomaly at reference time (semi-circles) [39], [49].  Scale factor 2-32 semi-circles. |
| ***bdsE***  Parameter e, Eccentricity [39], [49].  Scale factor 2-34. |
| ***bdsOmega***  Parameter  Argument of perigee (semi-circles) [39], [49].  Scale factor 2-32 semi-circles. |
| ***bdsOmega0***  Parameter0, Longitude of ascending node of orbital plane at weekly epoch (semi-circles) [39], [49].  Scale factor 2-32 semi-circles. |
| ***bdsI0***  Parameter i0, Inclination angle at reference time (semi-circles) [39], [49].  Scale factor 2-32 semi-circles. |
| ***bdsOmegaDot***  Parameter , Rate of right ascension (semi-circles/sec) [39], [49].  Scale factor 2-44 semi-circles/second. |
| ***bdsI0Dot***  Parameter i0dot, Rate of inclination angle (semi-circles/sec) [39], [49].  Scale factor 2-44 semi-circles/second. |
| ***bdsCuc***  Parameter Cuc, Amplitude of cosine harmonic correction to the argument of latitude (radians) [39], [49].  Scale factor 2-30 radians. |
| ***bdsCus***  Parameter Cus, Amplitude of sine harmonic correction to the argument of latitude (radians) [39], [49].  Scale factor 2-30 radians. |
| ***bdsCrc***  Parameter Crc, Amplitude of cosine harmonic correction term to the orbit radius (metres) [39], [49].  Scale factor 2-8 metres. |
| ***bdsCrs***  Parameter Crs, Amplitude of sine harmonic correction term to the orbit radius (metres) [39], [49].  Scale factor 2-8 metres. |
| ***bdsCic***  Parameter Cic, Amplitude of cosine harmonic correction term to the angle of inclination (radians) [39], [49].  Scale factor 2-30 radians. |
| ***bdsCis***  Parameter Cis, Amplitude of sine harmonic correction term to the angle of inclination (radians) [39], [49].  Scale factor 2-30 radians. |

#### – *NavModel-NavIC-KeplerianSet*

-- ASN1START

NavModel-NavIC-KeplerianSet-r16 ::= SEQUENCE {

navic-Toe-r16 INTEGER (0..65536),

navic-URAI-r16 INTEGER (0..15),

navic-W-r16 INTEGER (-2147483648..2147483647),

navic-DeltaN-r16 INTEGER (-2097152..2097151),

navic-M0-r16 INTEGER (-2147483648..2147483647),

navic-OmegaDot-r16 INTEGER (-2147483648..2147483647),

navic-E-r16 INTEGER (0..4294967295),

navic-IDot-r16 INTEGER (-8192..8191),

navic-APowerHalf-r16 INTEGER (0.. 4294967295),

navic-I0-r16 INTEGER (-2147483648..2147483647),

navic-Omega0-r16 INTEGER (-2147483648..2147483647),

navic-Crs-r16 INTEGER (-32768..32767),

navic-Cis-r16 INTEGER (-32768..32767),

navic-Cus-r16 INTEGER (-32768..32767),

navic-Crc-r16 INTEGER (-32768..32767),

navic-Cic-r16 INTEGER (-32768..32767),

navic-Cuc-r16 INTEGER (-32768..32767),

...

}

-- ASN1STOP

| *NavModel-NavIC-KeplerianSet* field descriptions |
| --- |
| ***navic-Toe***  Parameter toe, time-of-ephemeris in seconds [38].  Scale factor 24 seconds. |
| ***navic-URAI***  Parameter User Range Accuracy Index (in metres). This is a one-sigma estimate of the user range errors in the navigation data for the transmitting satellite as described under clause 6.2.1.4 in [38] |
| ***navic-W***  Parameter ω, argument of perigee (semi-circles) [38].  Scale factor 2-31 semi-circles. |
| ***navic-DeltaN***  Parameter n, mean motion difference from computed value (semi-circles/sec) [38]  Scale factor 2-41 semi-circles/second |
| ***navic-M0***  Parameter M0, mean anomaly at reference time (semi-circles) [38]  Scale factor 2-31 semi-circles. |
| ***navic-OmegaDot***  Parameter OMEGAdot, rate of change of right ascension (semi-circles/sec) [38]  Scale factor 2-41 semi-circles/second |
| ***navic-E***  Parameter e, eccentricity [38]  Scale factor 2-33. |
| ***navic-IDot***  Parameter Idot, rate of change of inclination angle (semi-circles/sec) [38]  Scale factor 2-43 semi-circles/second. |
| ***navic-APowerHalf***  Parameter sqrtA, square root of semi-major Axis in (metres)½ [38]  Scale factor 2-19 metres ½. |
| ***navic-I0***  Parameter i0, inclination angle at reference time (semi-circles) [38]  Scale factor 2-31 semi-circles. |
| ***navic-Omega0***  Parameter OMEGA0, longitude of ascending node of orbit plane at weekly epoch (semi-circles) [38]  Scale factor 2-31 semi-circles. |
| ***navic-Crs***  Parameter Crs, amplitude of the sine harmonic correction term to the orbit radius (metres) [38]  Scale factor 2-4 metres |
| ***navic-Cis***  Parameter Cis, amplitude of the sine harmonic correction term to the angle of inclination (radians) [38]  Scale factor 2-28 radians |
| ***navic-Cus***  Parameter Cus, amplitude of the sine harmonic correction term to the argument of latitude (radians) [38]  Scale factor 2-28 radians |
| ***navic-Crc***  Parameter Crc, amplitude of the cosine harmonic correction term to the orbit radius (metres) [38]  Scale factor 2-4 metres |
| ***navic-Cic***  Parameter Cic, amplitude of the cosine harmonic correction term to the angle of inclination (radians) [38]  Scale factor 2-28 radians |
| ***navic-Cuc***  Parameter Cuc, amplitude of the cosine harmonic correction term to the argument of latitude (radians) [38]  Scale factor 2-28 radians |

#### – *GNSS-RealTimeIntegrity*

The IE *GNSS-RealTimeIntegrity* is used by the location server to provide parameters that describe the real-time status of the GNSS constellations. *GNSS-RealTimeIntegrity* data communicates the health of the GNSS signals to the mobile in real‑time.

The location server always transmits the *GNSS-RealTimeIntegrity* with the current list of unhealthy signals (i.e., not only for signals/SVs currently visible at the reference location), for any GNSS positioning attempt and whenever GNSS assistance data are sent. If the number of bad signals is zero, then the *GNSS-RealTimeIntegrity* IE is omitted.

NOTE 1: If GNSS integrity assistance data are provided (i.e., any of *GNSS-Integrity-ServiceParameters*, *GNSS-Integrity-ServiceAlert*, *ORBIT-IntegrityParameters*, *SSR-IntegrityOrbitBounds*, *CLOCK-IntegrityParameters*, *SSR-IntegrityClockBounds*, *SSR-IntegrityCodeBiasBounds*, *SSR-IntegrityPhaseBiasBounds*, *STEC-IntegrityParameters*, *STEC-IntegrityErrorBounds*, *SSR-GriddedCorrectionIntegrityParameters*, *TropoDelayIntegrityErrorBounds*) the following interpretation of the IE *GNSS-RealTimeIntegrity* applies:

- Absence of the IE *GNSS-RealTimeIntegrity* indicates DNU=FALSE according to the Integrity Principle of Operation specified in clause 8.1.1a of TS 38.305 [40] for all GNSS satellites for which integrity assistance data are provided.

- Presence of the IE *GNSS-RealTimeIntegrity* for a GNSS satellite and signal combination indicates DNU=TRUE for this GNSS satellite and signal combination according to the Integrity Principle of Operation specified in clause 8.1.1a of TS 38.305 [40].

NOTE 2: The UE assumes that only those satellites for which the GNSS integrity assistance data are provided are monitored by the network and can be used for integrity related applications.

-- ASN1START

GNSS-RealTimeIntegrity ::= SEQUENCE {

gnss-BadSignalList GNSS-BadSignalList,

...

}

GNSS-BadSignalList ::= SEQUENCE (SIZE(1..64)) OF BadSignalElement

BadSignalElement ::= SEQUENCE {

badSVID SV-ID,

badSignalID GNSS-SignalIDs OPTIONAL, -- Need OP

...

}

-- ASN1STOP

| *GNSS-RealTimeIntegrity* field descriptions |
| --- |
| ***gnss-BadSignalList***  This field specifies a list of satellites with bad signal or signals. |
| ***badSVID***  This field specifies the GNSS *SV‑ID* of the satellite with bad signal or signals. |
| ***badSignalID***  This field identifies the bad signal or signals of a satellite. This is represented by a bit string in *GNSS-SignalIDs*, with a one‑value at a bit position means the particular GNSS signal type of the SV is unhealthy; a zero‑value means healthy. Absence of this field means that all signals on the specific SV are bad. |

#### – *GNSS-DataBitAssistance*

The IE *GNSS-DataBitAssistance* is used by the location server to provide data bit assistance data for specific satellite signals for data wipe-off. The data bits included in the assistance data depends on the GNSS and its signal.

-- ASN1START

GNSS-DataBitAssistance ::= SEQUENCE {

gnss-TOD INTEGER (0..3599),

gnss-TODfrac INTEGER (0..999) OPTIONAL, -- Need ON

gnss-DataBitsSatList GNSS-DataBitsSatList,

...

}

GNSS-DataBitsSatList ::= SEQUENCE (SIZE(1..64))OF GNSS-DataBitsSatElement

GNSS-DataBitsSatElement ::= SEQUENCE {

svID SV-ID,

gnss-DataBitsSgnList GNSS-DataBitsSgnList,

...

}

GNSS-DataBitsSgnList ::= SEQUENCE (SIZE(1..8)) OF GNSS-DataBitsSgnElement

GNSS-DataBitsSgnElement ::= SEQUENCE {

gnss-SignalType GNSS-SignalID,

gnss-DataBits BIT STRING (SIZE (1..1024)),

...

}

-- ASN1STOP

| *GNSS-DataBitAssistance* field descriptions |
| --- |
| ***gnss-TOD***  This field specifies the reference time of the first bit of the data in *GNSS-DataBitAssistance* in integer seconds in GNSS specific system time, modulo 1 hour.  Scale factor 1 second. |
| ***gnss-TODfrac***  This field specifies the fractional part of the *gnss-TOD* in 1‑milli‑second resolution.  Scale factor 1 millisecond. The total GNSS TOD is *gnss-TOD* + *gnss-TODfrac.* |
| ***gnss-DataBitsSatList***  This list specifies the data bits for a particular GNSS satellite *SV-ID* and signal *GNSS-SignalID*. |
| ***svID***  This field specifies the GNSS *SV‑ID* of the satellite for which the *GNSS-DataBitAssistance* is given. |
| ***gnss-SignalType***  This field identifies the GNSS signal type of the *GNSS-DataBitAssistance.* |
| ***gnss-DataBits***  Data bits are contained in GNSS system and data type specific format.  In the case of GPS L1 C/A, it contains the NAV data modulation bits as defined in [4] .  In the case of Modernized GPS L1C, it contains the encoded and interleaved modulation symbols as defined in [6] clause 3.2.3.1. In the case of Modernized GPS L2C, it contains either the NAV data modulation bits, the FEC encoded NAV data modulation symbols, or the FEC encoded CNAV data modulation symbols, dependent on the current signal configuration of this satellite as defined in [4, Table 3-III]. In the case of Modernized GPS L5, it contains the FEC encoded CNAV data modulation symbols as defined in [5].  In the case of SBAS, it contains the FEC encoded data modulation symbols as defined in [10].  In the case of QZSS QZS-L1, it contains the NAV data modulation bits as defined in [7] clause 5.2. In the case of QZSS QZS-L1C, it contains the encoded and interleaved modulation symbols as defined in [7] clause 5.3. In the case of QZSS QZS-L2C, it contains the encoded modulation symbols as defined in [7] clause 5.5. In the case of QZSS QZS-L5, it contains the encoded modulation symbols as defined in [7] clause 5.6.  In the case of GLONASS, it contains the 100 sps differentially Manchester encoded modulation symbols as defined in [9] clause 3.3.2.2.  In the case of Galileo, it contains the FEC encoded and interleaved modulation symbols. The logical levels 1 and 0 correspond to signal levels -1 and +1, respectively.  In the case of BDS B1I, it contains the encoded and interleaved modulation symbols as defined in [23], clause 5.1.3.  In the case of BDS B1C, it contains the encoded and interleaved modulation symbols as defined in [39], clause 6.2.2.  In the case of BDS B2a, it contains the encoded and interleaved modulation symbols as defined in [49], clause 6.2.2.  In the case of BDS B3I, it contains the encoded and interleaved modulation symbols as defined in [50], clause 5.1.3.  In the case of NavIC, it contains the FEC encoded and interleaved Navigation symbols as defined in [38]. |

#### – *GNSS-AcquisitionAssistance*

The IE *GNSS-AcquisitionAssistance* is used by the location server to provide parameters that enable fast acquisition of the GNSS signals. Essentially, these parameters describe the range and derivatives from respective satellites to the reference location at the reference time *GNSS-SystemTime* provided in IE *GNSS-ReferenceTime*.

Whenever *GNSS-AcquisitionAssistance* is provided by the location server, the IE *GNSS-ReferenceTime* is provided as well. E.g., even if the target device request for assistance data includes only a request for *GNSS-AcquisitionAssistance,* the location server also provides the corresponding IE *GNSS-ReferenceTime.*

Figure 6.5.2.2-1 illustrates the relation between some of the fields, using GPS TOW as exemplary reference.

-- ASN1START

GNSS-AcquisitionAssistance ::= SEQUENCE {

gnss-SignalID GNSS-SignalID,

gnss-AcquisitionAssistList GNSS-AcquisitionAssistList,

...,

confidence-r10 INTEGER (0..100) OPTIONAL -- Need ON

}

GNSS-AcquisitionAssistList ::= SEQUENCE (SIZE(1..64)) OF GNSS-AcquisitionAssistElement

GNSS-AcquisitionAssistElement ::= SEQUENCE {

svID SV-ID,

doppler0 INTEGER (-2048..2047),

doppler1 INTEGER (0..63),

dopplerUncertainty INTEGER (0..4),

codePhase INTEGER (0..1022),

intCodePhase INTEGER (0..127),

codePhaseSearchWindow INTEGER (0..31),

azimuth INTEGER (0..511),

elevation INTEGER (0..127),

...,

codePhase1023 BOOLEAN OPTIONAL, -- Need OP

dopplerUncertaintyExt-r10 ENUMERATED { d60,

d80,

d100,

d120,

noInformation, ... } OPTIONAL -- Need ON

}

-- ASN1STOP

| *GNSS-AcquisitionAssistance* field descriptions |
| --- |
| ***gnss-SignalID***  This field specifies the GNSS signal for which the acquisition assistance are provided. |
| ***gnss-AcquisitionAssistList***  These fields provide a list of acquisition assistance data for each GNSS satellite. |
| ***confidence***  This field specifies the confidence level of the reference location area or volume used to calculate the acquisition assistance parameters (search windows). A high percentage value (e.g., 98% or more) indicates to the target device that the provided search windows are reliable. The location server should include this field to indicate the confidence level of the provided information. |
| ***svID***  This field specifies the GNSS *SV‑ID* of the satellite for which the *GNSS-AcquisitionAssistance* is given. |
| ***doppler0***  This field specifies the Doppler (0th order term) value. A positive value in Doppler defines the increase in satellite signal frequency due to velocity towards the target device. A negative value in Doppler defines the decrease in satellite signal frequency due to velocity away from the target device. Doppler is given in unit of m/s by multiplying the Doppler value in Hz by the nominal wavelength of the assisted signal.  Scale factor 0.5 m/s in the range from -1024 m/s to +1023.5 m/s. |
| ***doppler1***  This field specifies the Doppler (1st order term) value. A positive value defines the rate of increase in satellite signal frequency due to acceleration towards the target device. A negative value defines the rate of decrease in satellite signal frequency due to acceleration away from the target device.  Scale factor 1/210 m/s2 in the range from -0.2 m/s2 to +0.1 m/s2.  Actual value of Doppler (1st order term) is calculated as (-42 + *doppler1*) \* 1/210 m/s2, with *doppler1* in the range of 0…63. |
| ***dopplerUncertainty***  This field specifies the Doppler uncertainty value. It is defined such that the Doppler experienced by a stationary target device is in the range [DopplerDoppler Uncertainty] to [DopplerDoppler Uncertainty]. Doppler Uncertainty is given in unit of m/s by multiplying the Doppler Uncertainty value in Hz by the nominal wavelength of the assisted signal.  Defined values: 2.5 m/s, 5 m/s, 10 m/s, 20 m/s, 40 m/s as encoded by an integer *n* in the range 0-4 according to:  2-n(40) m/s; n = 0 – 4.  If the *dopplerUncertaintyExt* field is present, the target device that supports the *dopplerUncertaintyExt* shall ignore this field. |
| ***codePhase***  This field together with the *codePhase1023* field specifies the code phase, in units of milli‑seconds, in the range from 0 to 1 millisecond scaled by the nominal chipping rate of the GNSS signal, where increasing values of the field signify increasing predicted signal code phases, as seen by a receiver at the reference location at the reference time. The reference location would typically be an *a priori* estimate of the target device location.  Scale factor 2-10 msin the range from 0 to (1-2-10) ms.  Note: The value (1-2-10) ms is encoded using the *codePhase1023* IE. |
| ***intCodePhase***  This field contains integer code phase (expressed modulo 128 ms). The satellite integer milli-seconds code phase currently being transmitted at the reference time, as seen by a receiver at the reference location is calculated as reference time (expressed in milli-seconds) minus (*intCodePhase* + (n×128 ms)), as shown in Figure 6.5.2.2-1, with n = …-2,-1,0,1,2….  Scale factor 1 msin the range from 0 to 127 ms. |
| ***codePhaseSearchWindow***  This field contains the code phase search window. The code phase search window accounts for the uncertainty in the estimated target device location but not any uncertainty in reference time. It is defined such that the expected code phase is in the range [Code PhaseCode Phase Search Window] to [Code PhaseCode Phase Search Window] given in units of milli‑seconds.  Range 0-31, mapping according to the table *codePhaseSearchWindow* Value to Code Phase Search Window [ms] relation shown below. |
| ***azimuth***  This field specifies the azimuth angle. An angle of x degrees means the satellite azimuth a is in the range  (x ≤ a < x+0.703125) degrees.  Scale factor 0.703125 degrees. |
| ***elevation***  This field specifies the elevation angle. An angle of y degrees means the satellite elevation e is in the range  (y ≤ e < y+0.703125) degrees.  Scale factor 0.703125 degrees. |
| ***codePhase1023***  This field if set to TRUE indicates that the code phase has the value 1023 × 2-10 = (1-2-10) ms. This field may only be set to TRUE if the value provided in the *codePhase* IE is 1022. If this field is set to FALSE, the code phase is the value provided in the *codePhase* IE in the range from 0 to (1 - 2×2-10) ms. If this field is not present and the *codePhase* IE has the value 1022, the target device may assume that the code phase is between (1 - 2×2-10) and (1 - 2-10) ms. |
| ***dopplerUncertaintyExt***  If this field is present, the target device that supports this field shall ignore the *dopplerUncertainty* field. The location server should include this field only if supported by the target device.  This field specifies the Doppler uncertainty value. It is defined such that the Doppler experienced by a stationary target device is in the range [DopplerDoppler Uncertainty] to [DopplerDoppler Uncertainty]. Doppler Uncertainty is given in unit of m/s by multiplying the Doppler Uncertainty value in Hz by the nominal wavelength of the assisted signal.  Enumerated values define 60 m/s, 80 m/s, 100 m/s, 120 m/s, and "No Information". |

*codePhaseSearchWindow* Value to Code Phase Search Window [ms] relation

|  |  |
| --- | --- |
| *codePhaseSearchWindow*  Value | Code Phase Search Window [ms] |
| '00000' | No information |
| '00001' | 0,002 |
| '00010' | 0,004 |
| '00011' | 0,008 |
| '00100' | 0,012 |
| '00101' | 0,016 |
| '00110' | 0,024 |
| '00111' | 0,032 |
| '01000' | 0,048 |
| '01001' | 0,064 |
| '01010' | 0,096 |
| '01011' | 0,128 |
| '01100' | 0,164 |
| '01101' | 0,200 |
| '01110' | 0,250 |
| '01111' | 0,300 |
| '10000' | 0,360 |
| '10001' | 0,420 |
| '10010' | 0,480 |
| '10011' | 0,540 |
| '10100' | 0,600 |
| '10101' | 0,660 |
| '10110' | 0,720 |
| '10111' | 0,780 |
| '11000' | 0,850 |
| '11001' | 1,000 |
| '11010' | 1,150 |
| '11011' | 1,300 |
| '11100' | 1,450 |
| '11101' | 1,600 |
| '11110' | 1,800 |
| '11111' | 2,000 |



Figure 6.5.2.2-1: Exemplary calculation of some GNSS Acquisition Assistance fields.

#### – *GNSS-Almanac*

The IE *GNSS-Almanac* is used by the location server to provide the coarse, long-term model of the satellite positions and clocks. The meaning of these parameters is defined in relevant ICDs of the particular GNSS and GNSS specific interpretations apply. For example, GPS and QZSS use the same model parameters but some parameters have a different interpretation [7]. *GNSS-Almanac* is useful for receiver tasks that require coarse accuracy, such as determining satellite visibility. The model is valid for up to a few weeks, typically. Since it is a long-term model, the field should be provided for all satellites available in the GNSS constellation (i.e., not only for SVs visible at the reference location and including SVs flagged as unhealthy in almanac). The *completeAlmanacProvided* field indicates whether or not the location server provided almanacs for the complete GNSS constellation.

-- ASN1START

GNSS-Almanac ::= SEQUENCE {

weekNumber INTEGER (0..255) OPTIONAL, -- Need ON

toa INTEGER (0..255) OPTIONAL, -- Need ON

ioda INTEGER (0..3) OPTIONAL, -- Need ON

completeAlmanacProvided BOOLEAN,

gnss-AlmanacList GNSS-AlmanacList,

...,

[[ toa-ext-v1240 INTEGER (256..1023) OPTIONAL, -- Need ON

ioda-ext-v1240 INTEGER (4..15) OPTIONAL -- Need ON

]],

[[

weekNumber-ext-r16 INTEGER (256..8191) OPTIONAL, -- Need ON

toa-ext2-r16 INTEGER (256..65535) OPTIONAL -- Need ON

]]

}

GNSS-AlmanacList ::= SEQUENCE (SIZE(1..64)) OF GNSS-AlmanacElement

GNSS-AlmanacElement ::= CHOICE {

keplerianAlmanacSet AlmanacKeplerianSet, -- Model-1

keplerianNAV-Almanac AlmanacNAV-KeplerianSet, -- Model-2

keplerianReducedAlmanac AlmanacReducedKeplerianSet, -- Model-3

keplerianMidiAlmanac AlmanacMidiAlmanacSet, -- Model-4

keplerianGLONASS AlmanacGLONASS-AlmanacSet, -- Model-5

ecef-SBAS-Almanac AlmanacECEF-SBAS-AlmanacSet,-- Model-6

...,

keplerianBDS-Almanac-r12 AlmanacBDS-AlmanacSet-r12, -- Model-7

keplerianNavIC-Almanac-r16 AlmanacNavIC-AlmanacSet-r16 -- Model-8

}

-- ASN1STOP

| *GNSS-Almanac* field descriptions |
| --- |
| ***weekNumber, weekNumber-ext***  This field specifies the almanac reference week number in GNSS specific system time to which the almanac reference time *toa* is referenced, modulo 256 weeks. Either *weekNumber* or *weekNumber-ext* is required for non-GLONASS GNSSs.  In the case of Galileo, the almanac reference week number WNa natively contains only the 2 LSB's [8], clause 5.1.10].  In the case of BDS B1C and BDS B2a,the almanac reference week number is defined in [39], 7.9.1 and [49], 7.9.1.  In the case of NavIC, the almanac reference week number is defined in [38]. |
| ***toa, toa-ext, toa-ext2***  In the cases that *GNSS-ID* does not indicate Galileo or NavIC, this field specifies the almanac reference time given in GNSS specific system time, in units of seconds with a scale factor of 212. *toa* is required for non-GLONASS GNSSs when the *toa-ext2* is not present.  In the case that *GNSS-ID* indicates Galileo, this field specifies the almanac reference time given in GNSS specific system time, in units of seconds with a scale factor of 600 seconds. Either *toa* or *toa-ext* is required for Galileo GNSS.  In the case that *GNSS-ID* indicates NavIC, this field specifies the almanac reference time given in GNSS specific system time, in units of seconds with a scale factor of 16 seconds [38]. Either *toa* or *toa-ext2* is required for NavIC GNSS. |
| ***ioda, ioda-ext***  This field specifies the issue of data*.* Either *ioda* or *ioda-ext* is required for Galileo GNSS. |
| ***completeAlmanacProvided***  If set to TRUE, the *gnss-AlmanacList* contains almanacs for the complete GNSS constellation indicated by *GNSS‑ID*. |
| ***gnss-AlmanacList***  This list contains the almanac model for each GNSS satellite in the GNSS constellation. |

#### – *AlmanacKeplerianSet*

-- ASN1START

AlmanacKeplerianSet ::= SEQUENCE {

svID SV-ID,

kepAlmanacE INTEGER (0..2047),

kepAlmanacDeltaI INTEGER (-1024..1023),

kepAlmanacOmegaDot INTEGER (-1024..1023),

kepSV-StatusINAV BIT STRING (SIZE (4)),

kepSV-StatusFNAV BIT STRING (SIZE (2)) OPTIONAL, -- Need ON

kepAlmanacAPowerHalf INTEGER (-4096..4095),

kepAlmanacOmega0 INTEGER (-32768..32767),

kepAlmanacW INTEGER (-32768..32767),

kepAlmanacM0 INTEGER (-32768..32767),

kepAlmanacAF0 INTEGER (-32768..32767),

kepAlmanacAF1 INTEGER (-4096..4095),

...

}

-- ASN1STOP

| *AlmanacKeplerianSet* field descriptions |
| --- |
| ***svID***  This field identifies the satellite for which the GNSS Almanac Model is given. |
| ***kepAlmanacE***  Parameter e, eccentricity, dimensionless [8].  Scale factor 2-16. |
| ***kepAlmanacDeltaI***  Parameter δi, inclination at reference time relative to i0=56°; semi-circles [8].  Scale factor 2-14 semi-circles. |
| ***kepAlmanacOmegaDot***  Parameter , rate of change of right ascension (semi-circles/sec) [8].  Scale factor 2-33 semi-circles/seconds. |
| ***kepSV-StatusINAV***  This field contains the I/NAV signal health status [8], clause 5.1.10 , E5bHS and E1-BHS, where E5bHS occupies the 2 MSBs in *kepSV-StatusINAV*, and E1-BHS the two LSBs. |
| ***kepSV-StatusFNAV***  This field contains the F/NAV signal health status [8], clause 5.1.10 ,E5aHS. If the target device is supporting multiple Galileo signals, the location server includes this field. |
| ***kepAlmanacAPowerHalf***  Parameter (a1/2), difference with respect to the square root of the nominal semi-major axis, (metres)1/2 [8].  Scale factor 2-9 metres½ . |
| ***kepAlmanacOmega0***  Parameter OMEGA0, longitude of ascending node of orbital plane at weekly epoch (semi-circles) [8].  Scale factor 2-15 semi-circles. |
| ***kepAlmanacW***  Parameter ω, argument of perigee (semi-circles) [8].  Scale factor 2-15 semi-circles. |
| ***kepAlmanacM0***  Parameter M0, mean anomaly at reference time (semi-circles) [8].  Scale factor 2-15 semi-circles. |
| ***kepAlmanacAF0***  Parameter af0, satellite clock correction bias, seconds [8].  Scale factor 2-19 seconds. |
| ***kepAlmanacAF1***  Parameter af1, satellite clock correction linear, sec/sec [8].  Scale factor 2-38 seconds/second. |

#### – *AlmanacNAV-KeplerianSet*

-- ASN1START

AlmanacNAV-KeplerianSet ::= SEQUENCE {

svID SV-ID,

navAlmE INTEGER (0..65535),

navAlmDeltaI INTEGER (-32768..32767),

navAlmOMEGADOT INTEGER (-32768..32767),

navAlmSVHealth INTEGER (0..255),

navAlmSqrtA INTEGER (0..16777215),

navAlmOMEGAo INTEGER (-8388608..8388607),

navAlmOmega INTEGER (-8388608..8388607),

navAlmMo INTEGER (-8388608..8388607),

navAlmaf0 INTEGER (-1024..1023),

navAlmaf1 INTEGER (-1024..1023),

...

}

-- ASN1STOP

| *AlmanacNAV-KeplerianSet* field descriptions |
| --- |
| ***svID***  This field identifies the satellite for which the GNSS Almanac Model is given. |
| ***navAlmE***  Parameter e, eccentricity, dimensionless [4,7].  Scale factor 2-21. |
| ***navAlmDeltaI***  Parameter δi, correction to inclination, semi-circles [4,7].  Scale factor 2-19 semi-circles. |
| ***navAlmOMEGADOT***  Parameter , rate of right ascension, semi-circles/sec [4,7].  Scale factor 2-38 semi-circles/second. |
| ***navAlmSVHealth***  Parameter SV Health, satellite health [4,7]. |
| ***navAlmSqrtA***  Parameter , square root of the semi-major axis, metres/2 [4,7]  Scale factor 2-11 metres/2. |
| ***navAlmOMEGAo***  Parameter 0, longitude of ascending node of orbit plane at weekly epoch, semi-circles [4,7].  Scale factor 2-23 semi-circles. |
| ***navAlmOmega***  Parameter ω, argument of perigee semi-circles [4,7].  Scale factor 2-23 semi-circles. |
| ***navAlmMo***  Parameter M0, mean anomaly at reference time semi-circles [4,7].  Scale factor 2-23 semi-circles. |
| ***navAlmaf0***  Parameter af0, apparent satellite clock correction seconds [4,7].  Scale factor 2-20 seconds. |
| ***navAlmaf1***  Parameter af1, apparent satellite clock correction sec/sec [4,7].  Scale factor 2-38 semi-circles seconds/second. |

#### – *AlmanacReducedKeplerianSet*

-- ASN1START

AlmanacReducedKeplerianSet ::= SEQUENCE {

svID SV-ID,

redAlmDeltaA INTEGER (-128..127),

redAlmOmega0 INTEGER (-64..63),

redAlmPhi0 INTEGER (-64..63),

redAlmL1Health BOOLEAN,

redAlmL2Health BOOLEAN,

redAlmL5Health BOOLEAN,

...

}

-- ASN1STOP

| *AlmanacReducedKeplerianSet* field descriptions |
| --- |
| ***svID***  This field identifies the satellite for which the GNSS Almanac Model is given. |
| ***redAlmDeltaA***  Parameter A, metres [4], [5], [6], [7], [39], [49].  Scale factor 2+9 metres. |
| ***redAlmOmega0***  Parameter 0, semi-circles [4], [5], [6], [7], [39], [49].  Scale factor 2-6 semi-circles. |
| ***redAlmPhi0***  Parameter 0, semi-circles [4], [5], [6], [7], [39], [49].  Scale factor 2-6 semi-circles. |
| ***redAlmL1Health***  Parameter L1 Health, dimensionless [4], [5], [6], [7].  If *GNSS-ID* = BDS, this field indicates the Satellite clock health state (the 8th bit) defined in table 7-14 [39] for BDS B1C and in table 7-14 [49] for BDS B2a. |
| ***redAlmL2Health***  Parameter L2 Health, dimensionless [4], [5], [6], [7].  If *GNSS-ID* = BDS, this field indicates the B1C signal health state (the 7th bit) defined in table 7-14 [39] for BDS B1C and in table 7-14 [49] for BDS B2a. |
| ***redAlmL5Health***  Parameter L5 Health, dimensionless [4], [5], [6], [7].  If *GNSS-ID* = BDS, this field indicates the B2a signal health state (the 6th bit) defined in table 7-14 [39] for BDS B1C and in table 7-14 [49] for BDS B2a. |

#### – *AlmanacMidiAlmanacSet*

-- ASN1START

AlmanacMidiAlmanacSet ::= SEQUENCE {

svID SV-ID,

midiAlmE INTEGER (0..2047),

midiAlmDeltaI INTEGER (-1024..1023),

midiAlmOmegaDot INTEGER (-1024..1023),

midiAlmSqrtA INTEGER (0..131071),

midiAlmOmega0 INTEGER (-32768..32767),

midiAlmOmega INTEGER (-32768..32767),

midiAlmMo INTEGER (-32768..32767),

midiAlmaf0 INTEGER (-1024..1023),

midiAlmaf1 INTEGER (-512..511),

midiAlmL1Health BOOLEAN,

midiAlmL2Health BOOLEAN,

midiAlmL5Health BOOLEAN,

...

}

-- ASN1STOP

| *AlmanacMidiAlmanacSet* field descriptions |
| --- |
| ***svID***  This field identifies the satellite for which the GNSS Almanac Model is given. |
| ***midiAlmE***  Parameter e, dimensionless [4], [5], [6], [7], [39], [49].  Scale factor 2-16. |
| ***midiAlmDeltaI***  Parameter i, semi-circles [4], [5], [6], [7], [39], [49].  Scale factor 2-14 semi-circles. |
| ***midiAlmOmegaDot***  Parameter , semi-circles/sec [4], [5], [6], [7], [39], [49].  Scale factor 2-33 semi-circles/second. |
| ***midiAlmSqrtA***  Parameter , metres1/2 [4], [5], [6], [7], [39], [49].  Scale factor 2-4 metres1/2. |
| ***midiAlmOmega0***  Parameter 0, semi-circles [4], [5], [6], [7], [39], [49].  Scale factor 2-15 semi-circles. |
| ***midiAlmOmega***  Parameter , semi-circles [4], [5], [6], [7], [39], [49].  Scale factor 2-15 semi-circles. |
| ***midiAlmMo***  Parameter M0, semi-circles [4], [5], [6], [7], [39, [49].  Scale factor 2-15 semi-circles. |
| ***midiAlmaf0***  Parameter afo, seconds [4], [5], [6], [7], [39], [49].  Scale factor 2-20 seconds. |
| ***midiAlmaf1***  Parameter af1, sec/sec [4], [5], [6], [7], [39], [49].  Scale factor 2-37 seconds/second. |
| ***midiAlmL1Health***  Parameter L1 Health, dimensionless [4], [5], [6], [7].  If *GNSS-ID* = BDS, this field indicates the satellite clock health state (the 8th bit) defined in table 7-14 [39] for BDS B1C and in table 7-14 [49] for BDS B2a. |
| ***midiAlmL2Health***  Parameter L2 Health, dimensionless [4], [5], [6], [7].  If *GNSS-ID* = BDS, this field indicates the B1C signal health state (the 7th bit) defined in table 7-14 [39] for BDS B1C and in table 7-14 [49] for BDS B2a. |
| ***midiAlmL5Health***  Parameter L5 Health, dimensionless [4], [5], [6], [7].  If *GNSS-ID* = BDS, this field indicates the B2a signal health state (the 6th bit) defined in table 7-14 [39] for BDS B1C and in table 7-14 [49] for BDS B2a. |

#### – *AlmanacGLONASS-AlmanacSet*

-- ASN1START

AlmanacGLONASS-AlmanacSet ::= SEQUENCE {

gloAlm-NA INTEGER (1..1461),

gloAlmnA INTEGER (1..24),

gloAlmHA INTEGER (0..31),

gloAlmLambdaA INTEGER (-1048576..1048575),

gloAlmtlambdaA INTEGER (0..2097151),

gloAlmDeltaIa INTEGER (-131072..131071),

gloAlmDeltaTA INTEGER (-2097152..2097151),

gloAlmDeltaTdotA INTEGER (-64..63),

gloAlmEpsilonA INTEGER (0..32767),

gloAlmOmegaA INTEGER (-32768..32767),

gloAlmTauA INTEGER (-512..511),

gloAlmCA INTEGER (0..1),

gloAlmMA BIT STRING (SIZE(2)) OPTIONAL, -- Need ON

...

}

-- ASN1STOP

| *AlmanacGLONASS-AlmanacSet* field descriptions |
| --- |
| ***gloAlm-NA***  Parameter NA, days [9].  Scale factor 1 days. |
| ***gloAlmnA***  Parameter nA, dimensionless [9]. |
| ***gloAlmHA***  Parameter HnA, dimensionless [9]. |
| ***gloAlmLambdaA***  Parameter nA, semi-circles [9].  Scale factor 2-20 semi-circles. |
| ***gloAlmtlambdaA***  Parameter tnA, seconds [9].  Scale factor 2-5 seconds. |
| ***gloAlmDeltaIa***  Parameter inA, semi-circles [9].  Scale factor 2-20 semi-circles. |
| ***gloAlmDeltaTA***  Parameter TnA, sec/orbit period [9].  Scale factor 2-9 seconds/orbit period. |
| ***gloAlmDeltaTdotA***  Parameter T\_DOTnA, sec/orbit period2 [9].  Scale factor 2-14 seconds/orbit period2. |
| ***gloAlmEpsilonA***  Parameter nA, dimensionless [9].  Scale factor 2-20. |
| ***gloAlmOmegaA***  Parameter nA, semi-circles [9].  Scale factor 2-15 semi-circles. |
| ***gloAlmTauA***  Parameter nA, seconds [9].  Scale factor 2-18 seconds. |
| ***gloAlmCA***  Parameter CnA, dimensionless [9]. |
| ***gloAlmMA***  Parameter MnA, dimensionless [9]. This parameter is present if its value is nonzero; otherwise it is not present. |

#### – *AlmanacECEF-SBAS-AlmanacSet*

-- ASN1START

AlmanacECEF-SBAS-AlmanacSet ::= SEQUENCE {

sbasAlmDataID INTEGER (0..3),

svID SV-ID,

sbasAlmHealth BIT STRING (SIZE(8)),

sbasAlmXg INTEGER (-16384..16383),

sbasAlmYg INTEGER (-16384..16383),

sbasAlmZg INTEGER (-256..255),

sbasAlmXgdot INTEGER (-4..3),

sbasAlmYgDot INTEGER (-4..3),

sbasAlmZgDot INTEGER (-8..7),

sbasAlmTo INTEGER (0..2047),

...

}

-- ASN1STOP

| *AlmanacECEF-SBAS-AlmanacSet* field descriptions |
| --- |
| ***sbasAlmDataID***  Parameter Data ID, dimensionless [10]. |
| ***svID***  This field identifies the satellite for which the GNSS Almanac Model is given. |
| ***sbasAlmHealth***  Parameter Health, dimensionless [10]. |
| ***sbasAlmXg***  Parameter XG, metres [10].  Scale factor 2600 metres. |
| ***sbasAlmYg***  Parameter YG, metres [10].  Scale factor 2600 metres. |
| ***sbasAlmZg***  Parameter ZG, metres [10].  Scale factor 26000 metres. |
| ***sbasAlmXgdot***  Parameter XG Rat-of-Change, metres/second [10].  Scale factor 10 metres/second. |
| ***sbasAlmYgDot***  Parameter YG Rate-of-Change, metres/second [10].  Scale factor 10 metres/second. |
| ***sbasAlmZgDot***  Parameter ZG Rate-of-Change, metres/second [10].  Scale factor 40.96 metres/second. |
| ***sbasAlmTo***  Parameter t0, seconds [10].  Scale factor 64 metres/second. |

#### – *AlmanacBDS-AlmanacSet*

-- ASN1START

AlmanacBDS-AlmanacSet-r12 ::= SEQUENCE {

svID SV-ID,

bdsAlmToa-r12 INTEGER (0..255) OPTIONAL, -- Cond NotSameForAllSV

bdsAlmSqrtA-r12 INTEGER (0..16777215),

bdsAlmE-r12 INTEGER (0..131071),

bdsAlmW-r12 INTEGER (-8388608..8388607),

bdsAlmM0-r12 INTEGER (-8388608..8388607),

bdsAlmOmega0-r12 INTEGER (-8388608..8388607),

bdsAlmOmegaDot-r12 INTEGER (-65536..65535),

bdsAlmDeltaI-r12 INTEGER (-32768..32767),

bdsAlmA0-r12 INTEGER (-1024..1023),

bdsAlmA1-r12 INTEGER (-1024..1023),

bdsSvHealth-r12 BIT STRING (SIZE(9)) OPTIONAL, -- Cond SV-ID

...

}

-- ASN1STOP

| Conditional presence | Explanation |
| --- | --- |
| *NotSameForAllSV* | This field may be present if the toa is not the same for all SVs; otherwise it is not present and the toa is provided in *GNSS-Almanac*. |
| *SV-ID* | This field is mandatory present if *SV-ID* is between 0 and 63; otherwise it is not present. |

| *AlmanacBDS-AlmanacSet* field descriptions |
| --- |
| ***svID***  This field identifies the satellite for which the GNSS Almanac Model is given. |
| ***bdsAlmToa***  Parameter toa, Almanac reference time (seconds) [23], [50].  Scale factor 212 seconds. |
| ***bdsAlmSqrtA***  Parameter A1/2, Square root of semi-major axis (metres1/2) [23], [50].  Scale factor 2-11 metres1/2. |
| ***bdsAlmE***  Parameter e, Eccentricity, dimensionless [23], [50].  Scale factor 2-21. |
| ***bdsAlmW***  Parameter , Argument of Perigee (semi-circles) [23], [50].  Scale factor 2-23 semi-circles. |
| ***bdsAlmM0***  Parameter M0, Mean anomaly at reference time (semi-circles) [23], [50].  Scale factor 2-23 semi-circles. |
| ***bdsAlmOmega0***  Parameter 0, Longitude of ascending node of orbital plane computed according to reference time (semi-circles) [23], [50].  Scale factor 2-23 semi-circles. |
| ***bdsAlmOmegaDot***  Parameter  Rate of right ascension (semi-circles/second) [23], [50].  Scale factor 2-38 semi-circles/second. |
| ***bdsAlmDeltaI***  Parameter i, Correction of orbit reference inclination at reference time (semi-circles) [23], [50].  Scale factor 2-19 semi-circles. |
| ***bdsAlmA0***  Parameter a0, Satellite clock bias (seconds) [23], [50].  Scale factor 2-20 seconds. |
| ***bdsAlmA1***  Parameter a1, Satellite clock rate (sec/sec) [23], [50].  Scale factor 2-38 seconds/seconds. |
| ***bdsSvHealth***  This field indicates satellites health information as defined in [23], [50] Table 5-16. The left most bit is the MSB. |

#### – *AlmanacNavIC-AlmanacSet*

The IE *AlmanacNavIC-AlmanacSet* is used for NavIC L5 as defined in [38].

-- ASN1START

AlmanacNavIC-AlmanacSet-r16 ::= SEQUENCE {

svID-r16 SV-ID,

navic-AlmToa-r16 INTEGER (0..65535) OPTIONAL, -- Cond NotSameForAllSV

navic-AlmE-r16 INTEGER (0..65535),

navic-AlmOMEGADOT-r16 INTEGER (-32768..32767),

navic-AlmSqrtA-r16 INTEGER (0..16777215),

navic-AlmOMEGAo-r16 INTEGER (-8388608..8388607),

navic-AlmOmega-r16 INTEGER (-8388608..8388607),

navic-AlmMo-r16 INTEGER (-8388608..8388607),

navic-Almaf0-r16 INTEGER (-1024..1023),

navic-Almaf1-r16 INTEGER (-1024..1023),

...,

[[

navicL5-i0-r16 INTEGER (-8388608..8388607) OPTIONAL -- Need ON

]]

}

-- ASN1STOP

| Conditional presence | Explanation |
| --- | --- |
| *NotSameForAllSV* | This field is optionally present, need ON, if the toa is not the same for all SVs; otherwise it is not present and the toa is provided in *GNSS-Almanac*. |

| *AlmanacNavIC-AlmanacSet* field descriptions |
| --- |
| ***svID***  This field identifies the satellite for which the Almanac model is given. |
| ***navic-AlmToa***  This field provides the time of almanac set [38].  Scale factor 16 seconds. |
| ***navic-AlmE***  Parameter e, eccentricity, dimensionless [38].  Scale factor 2-21. |
| ***navic-AlmOMEGADOT***  Parameter , rate of right ascension, semi-circles/sec [38].  Scale factor 2-38 semi-circles/second |
| ***navic-AlmSqrtA***  Parameter , square root of the semi-major axis, metres1/2 [38].  Scale factor 2-11 metres1/2. |
| ***navic-AlmOMEGAo***  Parameter 0, longitude of ascending node of orbit plane at weekly epoch, semi-circles [38].  Scale factor 2-23 semi-circles. |
| ***navic-AlmOmega***  Parameter ω, argument of perigee semi-circles [38].  Scale factor 2-23 semi-circles. |
| ***navic-AlmMo***  Parameter M0, mean anomaly at reference time semi-circles [38].  Scale factor 2-23 semi-circles. |
| ***navic-Almaf0***  Parameter af0, apparent satellite clock correction seconds [38].  Scale factor 2-20 seconds. |
| ***navic-Almaf1***  Parameter af1, apparent satellite clock correction sec/sec [38].  Scale factor 2-38 semi-circles seconds/second. |
| ***navicL5-i0***  Parameter I0, inclination (semi-circles) as described in clause 6 of [38].  Scale factor 2-23 semi-circles. |

#### – *GNSS-UTC-Model*

The IE *GNSS-UTC-Model* is used by the location server to provide several sets of parameters needed to relate GNSS system time to Universal Time Coordinate (UTC), as defined in [4], [5], [6], [7], [8], [9], [10], [23], [38], [39], [49].

The UTC time standard, UTC(k), is GNSS specific. E.g., if *GNSS-ID* indicates GPS, *GNSS-UTC-Model* contains a set of parameters needed to relate GPS system time to UTC(USNO); if *GNSS-ID* indicates QZSS, *GNSS-UTC-Model* contains a set of parameters needed to relate QZST to UTC(NICT); if *GNSS-ID* indicates GLONASS, *GNSS-UTC-Model* contains a set of parameters needed to relate GLONASS system time to UTC(RU); if *GNSS-ID* indicates SBAS, *GNSS-UTC-Model* contains a set of parameters needed to relate SBAS network time for the SBAS indicated by *SBAS-ID* to the UTC standard defined by the UTC Standard ID; if *GNSS-ID* indicates BDS, *GNSS-UTC-Model* contains a set of parameters needed to relate BDS system time to UTC (NTSC), where *UTC-ModelSet2* is used for BDS B1C and BDS B2a, and *UTC-ModelSet5* is used for BDS B1I; if the *GNSS-ID* indicates NavIC, the *GNSS-UTC-Model* contains a set of parameters needed to relate NavIC system time to the UTC (BIPM).

-- ASN1START

GNSS-UTC-Model ::= CHOICE {

utcModel1 UTC-ModelSet1, -- Model-1

utcModel2 UTC-ModelSet2, -- Model-2

utcModel3 UTC-ModelSet3, -- Model-3

utcModel4 UTC-ModelSet4, -- Model-4

...,

utcModel5-r12 UTC-ModelSet5-r12 -- Model-5

}

-- ASN1STOP

#### – *UTC-ModelSet1*

-- ASN1START

UTC-ModelSet1 ::= SEQUENCE {

gnss-Utc-A1 INTEGER (-8388608..8388607),

gnss-Utc-A0 INTEGER (-2147483648..2147483647),

gnss-Utc-Tot INTEGER (0..255),

gnss-Utc-WNt INTEGER (0..255),

gnss-Utc-DeltaTls INTEGER (-128..127),

gnss-Utc-WNlsf INTEGER (0..255),

gnss-Utc-DN INTEGER (-128..127),

gnss-Utc-DeltaTlsf INTEGER (-128..127),

...

}

-- ASN1STOP

| *UTC-ModelSet1* field descriptions |
| --- |
| ***gnss-Utc-A1***  Parameter A1, scale factor 2-50 seconds/second [4,7,8]. |
| ***gnss-Utc-A0***  Parameter A0, scale factor 2-30 seconds [4,7,8]. |
| ***gnss-Utc-Tot***  Parameter tot, scale factor 212 seconds [4,7,8]. |
| ***gnss-Utc-WNt***  Parameter WNt, scale factor 1 week [4,7,8]. |
| ***gnss-Utc-DeltaTls***  Parameter ΔtLS, scale factor 1 second [4,7,8]. |
| ***gnss-Utc-WNlsf***  Parameter WNLSF, scale factor 1 week [4,7,8]. |
| ***gnss-Utc-DN***  Parameter DN, scale factor 1 day [4,7,8]. |
| ***gnss-Utc-DeltaTlsf***  Parameter ΔtLSF, scale factor 1 second [4,7,8]. |

#### – *UTC-ModelSet2*

-- ASN1START

UTC-ModelSet2 ::= SEQUENCE {

utcA0 INTEGER (-32768..32767),

utcA1 INTEGER (-4096..4095),

utcA2 INTEGER (-64..63),

utcDeltaTls INTEGER (-128..127),

utcTot INTEGER (0..65535),

utcWNot INTEGER (0..8191),

utcWNlsf INTEGER (0..255),

utcDN BIT STRING (SIZE(4)),

utcDeltaTlsf INTEGER (-128..127),

...,

[[

utcWNlsf-ext-r16 INTEGER (256..8191) OPTIONAL -- Need ON

]]

}

-- ASN1STOP

| *UTC-ModelSet2* field descriptions |
| --- |
| ***utcA0***  Parameter A0-n, bias coefficient of GNSS time scale relative to UTC time scale (seconds) [4], [5], [6], [7], [38], [39], [49].  Scale factor 2-35 seconds. |
| ***utcA1***  Parameter A1-n, drift coefficient of GNSS time scale relative to UTC time scale (sec/sec) [4], [5], [6], [7], [38], [39], [49].  Scale factor 2-51 seconds/second. |
| ***utcA2***  Parameter A2-n, drift rate correction coefficient of GNSS time scale relative to UTC time scale (sec/sec2) [4], [5], [6], [7], [38], [39], [49].  Scale factor 2-68 seconds/second2. |
| ***utcDeltaTls***  Parameter ΔtLS, current or past leap second count (seconds) [4], [5], [6], [7], [38], [39], [49].  Scale factor 1 second. |
| ***utcTot***  Parameter tot, time data reference time of week (seconds) [4], [5], [6], [7], [38], [39], [49].  Scale factor 24 seconds. |
| ***utcWNot***  Parameter WNot, time data reference week number (weeks) [4], [5], [6], [7], [38], [39], [49].  Scale factor 1 week. |
| ***utcWNlsf, utcWNlsf-ext***  Parameter WNLSF, leap second reference week number (weeks) [4], [5], [6], [7], [38], [39], [49].  If the field *utcWNlsf-ext* is present, the field *utcWNlsf* shall be ignored by the receiver.  Scale factor 1 week. |
| ***utcDN***  Parameter DN, leap second reference day number (days) [4], [5], [6], [7], [38], [39], [49].  Scale factor 1 day. |
| ***utcDeltaTlsf***  Parameter ΔtLSF, current or future leap second count (seconds) [4], [5], [6], [7], [38], [39], [49].  Scale factor 1 second. |

#### – *UTC-ModelSet3*

-- ASN1START

UTC-ModelSet3 ::= SEQUENCE {

nA INTEGER (1..1461),

tauC INTEGER (-2147483648..2147483647),

b1 INTEGER (-1024..1023) OPTIONAL, -- Cond GLONASS-M

b2 INTEGER (-512..511) OPTIONAL, -- Cond GLONASS-M

kp BIT STRING (SIZE(2)) OPTIONAL, -- Cond GLONASS-M

...

}

-- ASN1STOP

| Conditional presence | Explanation |
| --- | --- |
| *GLONASS-M* | The field is mandatory present if GLONASS-M satellites are present in the current GLONASS constellation; otherwise it is not present. |

| *UTC-ModelSet3* field descriptions |
| --- |
| ***nA***  Parameter NA, calendar day number within four-year period beginning since the leap year (days) [9].  Scale factor 1 day. |
| ***tauC***  Parameter c, GLONASS time scale correction to UTC(SU) (seconds) [9].  Scale factor 2-31 seconds. |
| ***b1***  Parameter B1, coefficient to determine UT1 (seconds) [9].  Scale factor 2-10 seconds. |
| ***b2***  Parameter B2, coefficient to determine UT1 (seconds/msd) [9].  Scale factor 2-16 seconds/msd. |
| ***kp***  Parameter KP, notification of expected leap second correction (dimensionless) [9]. |

#### – *UTC-ModelSet4*

-- ASN1START

UTC-ModelSet4 ::= SEQUENCE {

utcA1wnt INTEGER (-8388608..8388607),

utcA0wnt INTEGER (-2147483648..2147483647),

utcTot INTEGER (0..255),

utcWNt INTEGER (0..255),

utcDeltaTls INTEGER (-128..127),

utcWNlsf INTEGER (0..255),

utcDN INTEGER (-128..127),

utcDeltaTlsf INTEGER (-128..127),

utcStandardID INTEGER (0..7),

...

}

-- ASN1STOP

| *UTC-ModelSet4* field descriptions |
| --- |
| ***utcA1wnt***  Parameter A1WNT, sec/sec ([10], Message Type 12).  Scale factor 2-50 seconds/second. |
| ***utcA0wnt***  Parameter A0WNT, seconds ([10], Message Type 12).  Scale factor 2-30 seconds. |
| ***utcTot***  Parameter tot, seconds ([10], Message Type 12).  Scale factor 212 seconds. |
| ***utcWNt***  Parameter WNt, weeks ([10], Message Type 12).  Scale factor 1 week. |
| ***utcDeltaTls***  Parameter ΔtLS, seconds ([10], Message Type 12).  Scale factor 1 second. |
| ***utcWNlsf***  Parameter WNLSF, weeks ([10], Message Type 12).  Scale factor 1 week. |
| ***utcDN***  Parameter DN, days ([10], Message Type 12).  Scale factor 1 day. |
| ***utcDeltaTlsf***  Parameter ΔtLSF, seconds ([10], Message Type 12).  Scale factor 1 second. |
| ***utcStandardID***  If *GNSS-ID* indicates 'sbas', this field indicates the UTC standard used for the SBAS network time indicated by *SBAS‑ID* to UTC relation as defined in the table Value of UTC Standard ID to UTC Standard relation shown below ([10], Message Type 12). |

Value of UTC Standard ID to UTC Standard relation

|  |  |
| --- | --- |
| Value of UTC Standard ID | UTC Standard |
| 0 | UTC as operated by the Communications Research Laboratory (CRL), Tokyo, Japan |
| 1 | UTC as operated by the National Institute of Standards and Technology (NIST) |
| 2 | UTC as operated by the U. S. Naval Observatory (USNO) |
| 3 | UTC as operated by the International Bureau of Weights and Measures (BIPM) |
| 4-7 | Reserved for future definition |

#### – *UTC-ModelSet5*

-- ASN1START

UTC-ModelSet5-r12 ::= SEQUENCE {

utcA0-r12 INTEGER (-2147483648..2147483647),

utcA1-r12 INTEGER (-8388608..8388607),

utcDeltaTls-r12 INTEGER (-128..127),

utcWNlsf-r12 INTEGER (0..255),

utcDN-r12 INTEGER (0..255),

utcDeltaTlsf-r12 INTEGER (-128..127),

...

}

-- ASN1STOP

| *UTC-ModelSet5* field descriptions |
| --- |
| ***utcA0***  Parameter A0UTC, BDS clock bias relative to UTC, seconds [23].  Scale factor 2-30 seconds. |
| ***utcA1***  Parameter A1UTC, BDS clock rate relative to UTC, sec/sec [23].  Scale factor 2-50 sec/sec. |
| ***utcDeltaTls***  Parameter ΔtLS, delta time due to leap seconds before the new leap second effective, seconds [23].  Scale factor 1 second. |
| ***utcWNlsf***  Parameter WNLSF, week number of the new leap second, weeks [23].  Scale factor 1 week. |
| ***utcDN***  Parameter DN, day number of week of the new leap second, days [23].  Scale factor 1 day. |
| ***utcDeltaTlsf***  Parameter ΔtLSF, delta time due to leap seconds after the new leap second effective, seconds [23].  Scale factor 1 second. |

#### – *GNSS-AuxiliaryInformation*

The IE *GNSS-AuxiliaryInformation* is used by the location server to provide additional information dependent on the *GNSS‑ID*. If *GNSS-AuxiliaryInformation* is provided together with other satellite dependent GNSS assistance data (i.e., any of *GNSS-DifferentialCorrections*, *GNSS-NavigationModel*, *GNSS-DataBitAssistance*, or *GNSS-AcquisitionAssistance* IEs), the *GNSS-AuxiliaryInformation* should be provided for the same satellites and in the same LPP message as the other satellite dependent GNSS assistance data.

-- ASN1START

GNSS-AuxiliaryInformation ::= CHOICE {

gnss-ID-GPS GNSS-ID-GPS,

gnss-ID-GLONASS GNSS-ID-GLONASS,

...,

[[ gnss-ID-BDS-r16 GNSS-ID-BDS-r16

]]

}

GNSS-ID-GPS ::= SEQUENCE (SIZE(1..64)) OF GNSS-ID-GPS-SatElement

GNSS-ID-GPS-SatElement ::= SEQUENCE {

svID SV-ID,

signalsAvailable GNSS-SignalIDs,

...

}

GNSS-ID-GLONASS ::= SEQUENCE (SIZE(1..64)) OF GNSS-ID-GLONASS-SatElement

GNSS-ID-GLONASS-SatElement ::= SEQUENCE {

svID SV-ID,

signalsAvailable GNSS-SignalIDs,

channelNumber INTEGER (-7..13) OPTIONAL, -- Cond FDMA

...

}

GNSS-ID-BDS-r16 ::= SEQUENCE (SIZE(1..64)) OF GNSS-ID-BDS-SatElement-r16

GNSS-ID-BDS-SatElement-r16 ::= SEQUENCE {

svID-r16 SV-ID,

satType-r16 INTEGER (0..3),

...

}

-- ASN1STOP

| Conditional presence | Explanation |
| --- | --- |
| *FDMA* | The field is mandatory present if the GLONASS SV indicated by *svID* broadcasts FDMA signals; otherwise it is not present. |

| *GNSS-AuxiliaryInformation* field descriptions |
| --- |
| ***gnss-ID-GPS***  This choice may only be present if *GNSS-ID* indicates GPS. |
| ***gnss-ID-GLONASS***  This choice may only be present if *GNSS-ID* indicates GLONASS. |
| ***gnss-ID-BDS***  This choice may only be present if *GNSS-ID* indicates BDS. |
| ***svID***  This field specifies the GNSS SV for which the *GNSS-AuxiliaryInformation* is given. |
| ***signalsAvailable***  This field indicates the ranging signals supported by the satellite indicated by *svID*. This field is given as a bit string as defined in *GNSS-SignalIDs* for a particular GNSS. If a bit is set to '1' it indicates that the satellite identified by *svID* transmits ranging signals according to the signal correspondence in *GNSS-SignalIDs*. If a bit is set to '0' it indicates that the corresponding signal is not supported on the satellite identified by *svID*. |
| ***channelNumber***  This field indicates the GLONASS carrier frequency number of the satellite identified by *svID*, as defined in [9]. |
| ***satType***  This field identifies the BDS B1C and BDS B2a Satellite orbit type, defined in [39], [49].  1 indicates the GEO satellite, 2 indicates the IGSO satellite, 3 indicates the MEO satellite, and 0 is reserved. |

#### – *BDS-DifferentialCorrections*

The IE *BDS-DifferentialCorrections* is used by the location server to provide differential corrections to the target device for BDS B1I and BDS B3I.

-- ASN1START

BDS-DifferentialCorrections-r12 ::= SEQUENCE {

dbds-RefTime-r12 INTEGER (0..3599),

bds-SgnTypeList-r12 BDS-SgnTypeList-r12,

...

}

BDS-SgnTypeList-r12 ::= SEQUENCE (SIZE (1..3)) OF BDS-SgnTypeElement-r12

BDS-SgnTypeElement-r12 ::= SEQUENCE {

gnss-SignalID GNSS-SignalID OPTIONAL, -- Need ON

dbds-CorrectionList-r12 DBDS-CorrectionList-r12,

...

}

DBDS-CorrectionList-r12 ::= SEQUENCE (SIZE (1..64)) OF DBDS-CorrectionElement-r12

DBDS-CorrectionElement-r12 ::= SEQUENCE {

svID SV-ID,

bds-UDREI-r12 INTEGER (0..15),

bds-RURAI-r12 INTEGER (0..15),

bds-ECC-DeltaT-r12 INTEGER (-4096..4095),

...

}

-- ASN1STOP

| *BDS-DifferentialCorrections* field descriptions |
| --- |
| ***dbds-RefTime***  This field *specifies* the time for which the differential corrections are valid, modulo 1 hour. d*bds-RefTime* is given in BDS system time.  Scale factor 1‑second. |
| ***bds-UDREI***  This field indicates user differential range error information by user differential range error index (UDREI) as defined in [23], [50], clause 5.3.3.8.2. |
| ***bds-RURAI***  This field indicates Regional User Range Accuracy (RURA) information by Regional User Range Accuracy Index (UDREI) as defined in [23], [50], clause 5.3.3.7. |
| ***bds-ECC***-***DeltaT***  This field indicates the BDS differential correction information which is expressed in equivalent clock correction (t). Add the value of t to the observed pseudo-range to correct the effect caused by the satellite clock offset and ephemeris error. Value -4096 means the t is not available.  The scale factor is 0.1 metre. |

#### – *BDS-GridModelParameter*

The IE *BDS-GridModelParameter* is used by the location server to provide Ionospheric Grid Information to the target device for BDS B1I and BDS B3I.

-- ASN1START

BDS-GridModelParameter-r12 ::= SEQUENCE {

bds-RefTime-r12 INTEGER (0..3599),

gridIonList-r12 GridIonList-r12,

...

}

GridIonList-r12 ::= SEQUENCE (SIZE (1..320)) OF GridIonElement-r12

GridIonElement-r12 ::= SEQUENCE {

igp-ID-r12 INTEGER (1..320),

dt-r12 INTEGER (0..511),

givei-r12 INTEGER (0..15) ,

...

}

-- ASN1STOP

| *BDS-GridModelParamater* field descriptions |
| --- |
| ***bds-RefTime***  This field specifies the time for which the grid model parameters are valid, modulo 1 hour. *bds-RefTime* is given in BDS system time.  Scale factor 1‑second. |
| ***gridIonList***  This list provides ionospheric grid point information for each grid point. Up to 16 instances are used in this version of the specification. The values 17 to 320 are reserved for future use. |
| ***igp-ID***  This field indicates the ionospheric grid point (IGP) number as defined in [23], [50], clause 5.3.3.9. |
| ***dt***  This field indicates dT as defined in [23], [50], clause 5.3.3.9.1, i.e. the vertical delay at the corresponding IGP indicated by *igp-ID*.  The scale factor is 0.125 metre. |
| ***givei***  This field indicates the Grid Ionospheric Vertical Error Index (GIVEI) which is used to describe the delay correction accuracy at ionospheric grid point indicated by *igp-ID*, the mapping between GIVEI and GIVE is defined in [23], [50], clause 5.3.3.9.2. |

#### *– GNSS-RTK-Observations*

The IE *GNSS-RTK-Observations* is used by the location server to provide GNSS reference station observables (pseudorange, phaserange, phaserange-rate (Doppler), and carrier-to-noise ratio) of the GNSS signals. Essentially, these parameters describe the range and derivatives from respective satellites to the reference station location provided in IE *GNSS-RTK-ReferenceStationInfo*.

The parameters provided in IE *GNSS-RTK-Observations* are used as specified for message type 1071-1127 in [30].

-- ASN1START

GNSS-RTK-Observations-r15 ::= SEQUENCE {

epochTime-r15 GNSS-SystemTime,

gnss-ObservationList-r15 GNSS-ObservationList-r15,

...

}

GNSS-ObservationList-r15 ::= SEQUENCE (SIZE(1..64)) OF GNSS-RTK-SatelliteDataElement-r15

GNSS-RTK-SatelliteDataElement-r15 ::= SEQUENCE{

svID-r15 SV-ID,

integer-ms-r15 INTEGER (0..254) OPTIONAL, -- Need ON

rough-range-r15 INTEGER (0..1023),

rough-phase-range-rate-r15 INTEGER (-8192..8191) OPTIONAL, -- Need ON

gnss-rtk-SatelliteSignalDataList-r15 GNSS-RTK-SatelliteSignalDataList-r15,

...

}

GNSS-RTK-SatelliteSignalDataList-r15 ::= SEQUENCE (SIZE(1..24)) OF

GNSS-RTK-SatelliteSignalDataElement-r15

GNSS-RTK-SatelliteSignalDataElement-r15 ::= SEQUENCE {

gnss-SignalID-r15 GNSS-SignalID,

fine-PseudoRange-r15 INTEGER (-524288..524287),

fine-PhaseRange-r15 INTEGER (-8388608..8388607),

lockTimeIndicator-r15 INTEGER (0..1023),

halfCycleAmbiguityIndicator-r15 BIT STRING (SIZE (1)),

carrier-to-noise-ratio-r15 INTEGER (0..1023) OPTIONAL, -- Need ON

fine-PhaseRangeRate-r15 INTEGER (-16384..16383) OPTIONAL, -- Need ON

...

}

-- ASN1STOP

| *GNSS-RTK-Observations* field descriptions |
| --- |
| ***epochTime***  This field specifies the epoch time of the observations. The *gnss-TimeID* in *GNSS SystemTime* shall be the same as the *GNSS-ID* in IE *GNSS-GenericAssistDataElement.* |
| ***svID***  This field specifies the GNSS *SV‑ID* of the satellite for which the GNSS Observations are provided. |
| ***integer-ms***  This field contains the integer number of milliseconds in the satellite rough range. Rough range can be used to restore complete observables for a given satellite.  Scale factor 1 milli-second in the range from 0 to 254 milli-seconds. |
| ***rough-range***  This field contains the sub-milliseconds in the satellite rough range (modulo 1 millisecond).  Scale factor 2-10 milli-seconds in the range from 0 to (1-2-10) milli-seconds. |
| ***rough-phase-range-rate***  This field contains the GNSS satellite rough phaserange rate.  Scale factor 1 m/s. Range ±8191 m/s. |
| ***gnss-SignalID***  This field specifies the GNSS signal for which the GNSS observations are provided. |
| ***fine-PseudoRange***  This field contains the GNSS signal fine pseudorange.  Full pseudorange corresponding to the given signal is the sum of this field and the fields *integer-ms* and *rough-range*. NOTE 1.  Scale factor 2–29 milli-seconds. Range ±(2–10–2–29) milli-seconds. |
| ***fine-PhaseRange***  This field contains the GNSS signal fine phaserange.  Being added to fields *integer-ms* and *rough-range* allows getting the full phaserange observable corresponding to given signal. NOTE 2.  Scale factor 2–31 milli-seconds. Range ±(2–8–2–31) milli-seconds. |
| ***lockTimeIndicator***  This field provides a measure of the amount of time during which the receiver has maintained continuous lock on that satellite signal. If a cycle slip occurs during the previous measurement cycle, the lock time indicator shall be reset to zero.  The mapping of lock-time parameters as defined in [30] is according to the table *lockTimeIndicator* value to lock-time parameters relation shown below. |
| ***halfCycleAmbiguityIndicator***  Value 0 indicates no half-cycle ambiguity. Value 1 indicates half-cycle ambiguity.  When providing phaserange with unresolved polarity encoding this bit shall be set to 1. A target device that is not capable of handling half-cycle ambiguities shall skip such phaserange observables. If polarity resolution forced phaserange to be corrected by half-a-cycle, then the *lockTimeIndicator* must be reset to zero, indicating that despite continuous tracking the final phaserange experienced non-continuity. |
| ***carrier-to-noise-ratio***  This field provides the GNSS signal carrier-to-noise-ratio in dB-Hz.  Scale factor 2–4 dB-Hz in the range from 0.0625 to 63.9375 dB-Hz. |
| ***fine-PhaseRangeRate***  This field contains the GNSS signal fine Phase Range Rate.  Full phaserange rate is the sum of this field and the *rough-phase-range-rate* field. NOTE 3.  Scale factor 0.0001 m/s. Range ±1.6383 m/s. |

NOTE 1: Complete Pseudorange for each signal (i) of given satellite can be restored as follows:   
Pseudorange(i) = c/1000 × (*integer-ms* + *rough\_range*/1024 + 2–29 × *fine\_Pseudorange*(i)), metre.

NOTE 2: Complete Phaserange for each signal (i) of given satellite can be restored as follows:  
Phaserange(i) = c/1000 × (*integer-ms* + *rough\_range*/1024 + 2–31 × *fine\_Phaserange*(i)), metre.

NOTE 3: Complete PhaseRangeRate for each signal (i) of given satellite can be restored as follows:  
PhaseRangeRate(i) = *rough-phase-range-rate* + 0.0001\**fine-PhaseRangeRate* (i), metre/second.

NOTE 4: The speed of light c is 299,792,458 metres per second.

*lockTimeIndicator* value to lock-time parameters relation

|  |  |  |  |
| --- | --- | --- | --- |
| *lockTimeIndicator* value (i) | Supplementary coefficient (k) [30] | Minimum Lock Time (ms) [30] | Range of Indicated Lock Times (t) (ms) [30] |
| 0 – 63 | 1 | i | 0 ≤ t < 64 |
| 64 – 95 | 2 | 2 × i – 64 | 64 ≤ t < 128 |
| 96 – 127 | 4 | 4 × i – 256 | 128 ≤ t < 256 |
| 128 – 159 | 8 | 8 × i – 768 | 256 ≤ t < 512 |
| 160 – 191 | 16 | 16 × i – 2048 | 512 ≤ t < 1024 |
| 192 – 223 | 32 | 32 × i – 5120 | 1024 ≤ t < 2048 |
| 224 – 255 | 64 | 64 × i – 12288 | 2048 ≤ t < 4096 |
| 256 – 287 | 128 | 128 × i – 28672 | 4096 ≤ t < 8192 |
| 288 – 319 | 256 | 256 × i – 65536 | 8192 ≤ t < 16384 |
| 320 – 351 | 512 | 512 × i – 147456 | 16384 ≤ t < 32768 |
| 352 – 383 | 1024 | 1024 × i – 327680 | 32768 ≤ t < 65536 |
| 384 – 415 | 2048 | 2048 × i – 720896 | 65536 ≤ t < 131072 |
| 416 – 447 | 4096 | 4096 × i – 1572864 | 131072 ≤ t < 262144 |
| 448 – 479 | 8192 | 8192 × i – 3407872 | 262144 ≤ t < 524288 |
| 480 – 511 | 16384 | 16384 × i – 7340032 | 524288 ≤ t < 1048576 |
| 512 – 543 | 32768 | 32768 × i – 15728640 | 1048576 ≤ t < 2097152 |
| 544 – 575 | 65536 | 65536 × i – 33554432 | 2097152 ≤ t < 4194304 |
| 576 – 607 | 131072 | 131072 × i – 71303168 | 4194304 ≤ t < 8388608 |
| 608 – 639 | 262144 | 262144 × i – 150994944 | 8388608 ≤ t < 16777216 |
| 640 – 671 | 524288 | 524288 × i – 318767104 | 16777216 ≤ t < 33554432 |
| 672 – 703 | 1048576 | 1048576 × i – 671088640 | 33554432 ≤ t < 67108864 |
| 704 | 2097152 | 2097152 × i – 1409286144 | 67108864 ≤ t |
| 705 – 1023 | Reserved | | |

#### *– GLO-RTK-BiasInformation*

The IE *GLO-RTK-BiasInformation* is used by the location server to provide the so-called "GLONASS Code-Phase bias values" (CPB) for up to all FDMA GLONASS observations.

If IE *GNSS-RTK-Observations* for *gnss-ID* = *glonass* are provided, but IE *GLO-RTK-BiasInformation* is not provided, the target device assumes that the CPB information has been applied to the GLONASS observation data a priori.

The parameters provided in IE *GLO-RTK-BiasInformation* are used as specified for message type 1230 in [30].

-- ASN1START

GLO-RTK-BiasInformation-r15 ::= SEQUENCE{

referenceStationID-r15 GNSS-ReferenceStationID-r15,

cpbIndicator-r15 BIT STRING (SIZE(1)),

l1-ca-cpBias-r15 INTEGER (-32768..32767) OPTIONAL, -- Need ON

l1-p-cpBias-r15 INTEGER (-32768..32767) OPTIONAL, -- Need ON

l2-ca-cpBias-r15 INTEGER (-32768..32767) OPTIONAL, -- Need ON

l2-p-cpBias-r15 INTEGER (-32768..32767) OPTIONAL, -- Need ON

...

}

-- ASN1STOP

| *GLO-RTK-BiasInformation* field descriptions |
| --- |
| ***referenceStationID***  This field specifies the Station ID for which the *GLO-RTK-BiasInformation* is provided. |
| ***cpbIndicator***  This field specifies the GLONASS Code-Phase Bias Indicator. The interpretation of the value is as follows:  0 – The GLONASS Pseudorange and Phaserange observations in IE *GNSS-RTK-Observations* are not aligned to the same measurement epoch.  1 – The GLONASS Pseudorange and Phaserange observations in IE *GNSS-RTK-Observations* are aligned to the same measurement epoch. |
| ***l1-ca-cpBias***  This field specifies the GLONASS L1 C/A Code-Phase Bias, which represents the offset between the L1 C/A Pseudorange and L1 Phaserange measurement epochs in metres.  If *cpbIndicator* is set to 0, the measurement epoch of the GLONASS L1 Phaserange measurements may be aligned using:  Aligned GLONASS L1 Phaserange = Full GLONASS L1 Phaserange + GLONASS L1 C/A Code-Phase Bias.  If *cpbIndicator* is set to 1, the measurement epoch of the GLONASS L1 Phaserange measurements may be unaligned using:  Unaligned GLONASS L1 Phaserange = Full GLONASS L1 Phaserange – GLONASS L1 C/A Code-Phase Bias.  Scale factor 0.02 m. Range ±655.34 m. |
| ***l1-p-cpBias***  This field specifies the GLONASS L1 P Code-Phase Bias, which represents the offset between the L1 P Pseudorange and L1 Phaserange measurement epochs in metres.  If *cpbIndicator* is set to 0, the measurement epoch of the GLONASS L1 Phaserange measurements may be aligned using:  Aligned GLONASS L1 Phaserange = Full GLONASS L1 Phaserange + GLONASS L1 P Code-Phase Bias.  If *cpbIndicator* is set to 1, the measurement epoch of the GLONASS L1 Phaserange measurements may be unaligned using:  Unaligned GLONASS L1 Phaserange = Full GLONASS L1 Phaserange – GLONASS L1 P Code-Phase Bias.  Scale factor 0.02 m. Range ±655.34 m. |
| ***l2-ca-cpBias***  This field specifies the GLONASS L2 C/A Code-Phase Bias, which represents the offset between the L2 C/A Pseudorange and L2 Phaserange measurement epochs in metres.  If *cpbIndicator* is set to 0, the measurement epoch of the GLONASS L2 Phaserange measurements may be aligned using:  Aligned GLONASS L2 Phaserange = Full GLONASS L2 Phaserange + GLONASS L2 C/A Code-Phase Bias.  If *cpbIndicator* is set to 1, the measurement epoch of the GLONASS L2 Phaserange measurements may be unaligned using:  Unaligned GLONASS L2 Phaserange = Full GLONASS L2 Phaserange – GLONASS L2 C/A Code-Phase Bias.  Scale factor 0.02 m. Range ±655.34 m. |
| ***l2-p-cpBias***  This field specifies the GLONASS L2 P Code-Phase Bias, which represents the offset between the L2 P Pseudorange and L2 Phaserange measurement epochs in metres.  If *cpbIndicator* is set to 0, the measurement epoch of the GLONASS L2 Phaserange measurements may be aligned using:  Aligned GLONASS L2 Phaserange = Full GLONASS L2 Phaserange + GLONASS L2 P Code-Phase Bias.  If *cpbIndicator* is set to 1, the measurement epoch of the GLONASS L2 Phaserange measurements may be unaligned using:  Unaligned GLONASS L2 Phaserange = Full GLONASS L2 Phaserange – GLONASS L2 P Code-Phase Bias.  Scale factor 0.02 m. Range ±655.34 m. |

#### *– GNSS-RTK-MAC-CorrectionDifferences*

The IE *GNSS-RTK-MAC-CorrectionDifferences* is used by the location server to provide dispersive (ionospheric) and non-dispersive (geometric) correction difference components for up to 32 pairs of Auxiliary and Master Reference Stations. The Master Reference Station coordinates are provided in IE *GNSS-RTK-ReferenceStationInfo* and the Auxiliary Station coordinates are provided in IE *GNSS-RTK-AuxiliaryStationData*.

The parameters provided in IE *GNSS-RTK-MAC-CorrectionDifferences* are used as specified for message type 1017 and 1039 in [30] and apply to all GNSSs.

-- ASN1START

GNSS-RTK-MAC-CorrectionDifferences-r15 ::= SEQUENCE {

networkID-r15 GNSS-NetworkID-r15,

subNetworkID-r15 GNSS-SubNetworkID-r15 OPTIONAL, -- Need ON

master-ReferenceStationID-r15 GNSS-ReferenceStationID-r15,

l1-r15 GNSS-FrequencyID-r15 OPTIONAL, -- Need OP

l2-r15 GNSS-FrequencyID-r15 OPTIONAL, -- Need OP

rtkCorrectionDifferencesList-r15 RTK-CorrectionDifferencesList-r15,

...

}

RTK-CorrectionDifferencesList-r15 ::= SEQUENCE (SIZE (1..32)) OF

RTK-CorrectionDifferencesElement-r15

RTK-CorrectionDifferencesElement-r15 ::= SEQUENCE {

epochTime-r15 GNSS-SystemTime,

auxiliary-referenceStationID-r15 GNSS-ReferenceStationID-r15,

geometric-ionospheric-corrections-differences-r15

Geometric-Ionospheric-Corrections-Differences-r15,

...

}

Geometric-Ionospheric-Corrections-Differences-r15 ::= SEQUENCE (SIZE(1..64)) OF

Geometric-Ionospheric-Corrections-Differences-Element-r15

Geometric-Ionospheric-Corrections-Differences-Element-r15 ::= SEQUENCE {

svID-r15 SV-ID,

ambiguityStatusFlag-r15 INTEGER (0..3),

non-synch-count-r15 INTEGER (0..7),

geometricCarrierPhaseCorrectionDifference-r15 INTEGER (-65536..65535),

iod-r15 BIT STRING (SIZE(11)),

ionosphericCarrierPhaseCorrectionDifference-r15 INTEGER (-65536..65535),

...

}

-- ASN1STOP

| *GNSS-RTK-MAC-CorrectionDifferences* field descriptions |
| --- |
| ***networkID***  This field provides the network ID. |
| ***subNetworkID***  This field identifies the subnetwork of a network identified by *networkID*. |
| ***master-ReferenceStationID***  This field specifies the station ID of the Master Reference Station. |
| ***l1, l2***  These fields specify the dual-frequency combination of L1 and L2 link/frequencies for which the *rtkCorrectionDifferencesList* is provided. If the fields are absent, the default interpretation in table 'L1/L2 default interpretation' applies. |
| ***rtkCorrectionDifferencesList***  This field provides the correction differences for Auxiliary-Master Reference Station pairs. |
| ***epochTime***  This field specifies the epoch time of observations used to derive the correction differences. The *gnss-TimeID* in *GNSS‑SystemTime* shall be the same as the *GNSS-ID* in IE *GNSS-GenericAssistDataElement*. |
| ***auxiliary-referenceStationID***  This field specifies the station ID of the Auxiliary Reference Station. |
| ***svID***  This field specifies the satellite for which the data is provided. |
| ***ambiguityStatusFlag***  This field provides the ambiguity status. 'L1' below corresponds to the link indicated by the *l1* field; 'L2' below corresponds to the link indicated by the *l2* field.  0 - Reserved for future use (artificial observations)  1 - Correct Integer Ambiguity Level for L1 and L2  2 - Correct Integer Ambiguity Level for L1-L2 widelane  3 - Uncertain Integer Ambiguity Level. Only a likely guess is used. |
| ***non-synch-count***  This field provides the count of unrecoverable cycle slips. Whenever an unrecoverable cycle slip occurs this count shall be increased. The counter shall not be increased more than once per minute. Data for satellites with cycle slips more frequent than once per minute should not be provided. |
| ***geometricCarrierPhaseCorrectionDifference***  This field provides the Geometric Carrier Phase Correction Difference (GCPCD), which is the Correction Difference for the geometric part (troposphere and orbits) calculated based on integer leveled L1 and L2 correction differences (L1CD and L2CD).    L1CD, L2CD, and ICPCD are presented in metres. 'L1' below corresponds to the link indicated by the *l1* field; 'L2' below corresponds to the link indicated by the *l2* field.  Scale factor 0.5 millimetre; range ±32.767 metres. |
| ***iod***  This field specifies the IOD value of the broadcast ephemeris used for calculation of Correction Differences (see IE *GNSS-NavigationModel*). |
| ***ionosphericCarrierPhaseCorrectionDifference***  This field provides the Ionospheric Carrier Phase Correction Difference (ICPCD), which is the Correction Difference for the ionospheric part calculated based on integer leveled L1 and L2 correction differences (L1CD and L2CD).    L1CD, L2CD, and ICPCD are presented in metres. 'L1' below corresponds to the link indicated by the *l1* field; 'L2' below corresponds to the link indicated by the *l2* field.  Scale factor 0.5 millimetre; range ±32.767 metres. |

L1/L2 default interpretation

|  |  |  |
| --- | --- | --- |
| GNSS | *l1* | *l2* |
| GPS | L1 | L2 |
| SBAS | L1 | L5 |
| QZSS | L1 | L2 |
| Galileo | E1 | E5a |
| GLONASS | G1 | G2 |
| BDS | B1 | B2 |

#### *– GNSS-RTK-Residuals*

The IE *GNSS-RTK-Residuals* is used by the location server to provide Network RTK correction residual error information.

If the interpolation of the corrections for the target device location is performed at the location server, resulting in a non-physical reference station, the *GNSS-RTK-Residuals* are referenced to the non-physical reference station.

If the interpolation of the corrections is performed by the target device (e.g., using *GNSS‑RTK‑MAC‑CorrectionDifferences)*, the *GNSS-RTK-Residuals* are referenced to the closest master or auxiliary station to the target device.

The parameters provided in IE *GNSS-RTK-Residuals* are used as specified for message type 1030 and 1031 in [30] and apply to all GNSSs.

-- ASN1START

GNSS-RTK-Residuals-r15 ::= SEQUENCE {

epochTime-r15 GNSS-SystemTime,

referenceStationID-r15 GNSS-ReferenceStationID-r15,

n-Refs-r15 INTEGER (0..127),

l1-r15 GNSS-FrequencyID-r15 OPTIONAL, -- Need OP

l2-r15 GNSS-FrequencyID-r15 OPTIONAL, -- Need OP

rtk-residuals-list-r15 RTK-Residuals-List-r15,

...

}

RTK-Residuals-List-r15 ::= SEQUENCE (SIZE(1..64)) OF RTK-Residuals-Element-r15

RTK-Residuals-Element-r15 ::= SEQUENCE {

svID-r15 SV-ID,

s-oc-r15 INTEGER (0..255),

s-od-r15 INTEGER (0..511),

s-oh-r15 INTEGER (0..63),

s-lc-r15 INTEGER (0..1023),

s-ld-r15 INTEGER (0..1023),

...

}

-- ASN1STOP

| *GNSS-RTK-Residuals* field descriptions |
| --- |
| ***epochTime***  This field specifies the epoch time of the Network RTK Residual Error data. The *gnss-TimeID* in *GNSS‑SystemTime* shall be the same as the *GNSS-ID* in IE *GNSS-GenericAssistDataElement*. |
| ***referenceStationID***  This field specifies the Reference Station ID. The Reference Station may be a physical or non-physical station. |
| ***n-Refs***  This field specifies the number of reference stations used to derive the residual statistics (1 to 127; 127 indicates 127 or more stations). The number of reference stations should never be zero. If zero is encountered the target device should ignore the message. |
| ***l1, l2***  These fields specify the dual-frequency combination of L1 and L2 link/frequencies for which the *rtk residuals-list* is provided. If the fields are absent, the default interpretation in table 'L1/L2 default interpretation' in IE *GNSS‑RTK‑MAC‑CorrectionDifferences* applies. |
| **svID**  This field specifies the satellite for which the data is provided. |
| ***s-oc***  This field specifies the constant term of standard deviation (1 sigma) for non-dispersive interpolation residuals, *s0c*.  Scale factor 0.5 millimetre; range 0–127 millimetre. NOTE 1. |
| ***s-od***  This field specifies the distance dependent term of standard deviation (1 sigma) for nondispersive interpolation residuals, *s0d*.  Scale factor 0.01 ppm; range 0–5.11 ppm. NOTE 1. |
| ***s-oh***  This field specifies the height dependent term of standard deviation (1 sigma) for nondispersive interpolation residuals, *s0h*.  Scale factor 0.1 ppm; range 0–5.1 ppm. NOTE 1. |
| ***s-lc***  This field specifies the constant term of standard deviation (1 sigma) for dispersive interpolation residuals (as affecting L1 frequency), *slc*. 'L1' corresponds to the link indicated by the *l1* field.  Scale factor 0.5 millimetre; range 0–511 millimetre |
| ***s-ld***  This field specifies the distance dependent term of standard deviation (1 sigma) for dispersive interpolation residuals (as affecting L1 frequency), *sld*. 'L1' corresponds to the link indicated by the *l1* field. NOTE 2. |

NOTE 1: The complete standard deviation for the expected non-dispersive interpolation residual is computed from *s-oc*, *s-od* and *s-oh* using the formula:  
  
where *dRef* is the distance of the target device from the nearest physical reference station in [km] and |*dhRef*| is the absolute value of the height difference between the nearest physical reference station and the target device in [km].

NOTE 2: The complete standard deviation for the expected dispersive interpolation residual is computed from *s-lc* and *s-ld* using the formula:  
  
where *dRef* is the distance of the target device from the nearest physical reference station in [km].   
The standard deviation for the L2 frequency is calculated using the formula:  
. 'L2' corresponds to the link indicated by the *l2* field; *c/f1c/f2* are the nominal wavelengths of the links indicated by the *l1*, *l2* fields, respectively.

#### *– GNSS-RTK-FKP-Gradients*

The IE *GNSS-RTK-FKP-Gradients* is used by the location server to provide the FKP Network RTK gradients of distance-dependent errors like ionosphere, troposphere and orbits. The target device may use the gradients to compute the influence of the distance dependent errors for its own position.

The parameters provided in IE *GNSS-RTK-FKP-Gradients* are used as specified for message type 1034 and 1035 in [30] and apply to all GNSSs.

-- ASN1START

GNSS-RTK-FKP-Gradients-r15 ::= SEQUENCE {

referenceStationID-r15 GNSS-ReferenceStationID-r15,

epochTime-r15 GNSS-SystemTime,

l1-r15 GNSS-FrequencyID-r15 OPTIONAL, -- Need OP

l2-r15 GNSS-FrequencyID-r15 OPTIONAL, -- Need OP

fkp-gradients-list-r15 FKP-Gradients-List-r15,

...

}

FKP-Gradients-List-r15 ::= SEQUENCE (SIZE(1..64)) OF FKP-Gradients-Element-r15

FKP-Gradients-Element-r15 ::= SEQUENCE {

svID-r15 SV-ID,

iod-r15 BIT STRING (SIZE(11)),

north-geometric-gradient-r15 INTEGER (-2048..2047),

east-geometric-gradient-r15 INTEGER (-2048..2047),

north-ionospheric-gradient-r15 INTEGER (-8192..8191),

east-ionospheric-gradient-r15 INTEGER (-8192..8191),

...

}

-- ASN1STOP

| *GNSS-RTK-FKP-Gradients* field descriptions |
| --- |
| ***referenceStationID***  This field specifies the Reference Station ID. The Reference Station may be a physical or non-physical station. |
| ***epochTime***  This field specifies the epoch time of the FKP data. The *gnss-TimeID* in *GNSS‑SystemTime* shall be the same as the *GNSS-ID* in IE *GNSS-GenericAssistDataElement*. |
| ***l1, l2***  These fields specify the dual-frequency combination of L1 and L2 link/frequencies for which the *fkp-gradients-list* is provided. If the fields are absent, the default interpretation in table 'L1/L2 default interpretation' in IE *GNSS‑RTK‑MAC‑CorrectionDifferences* applies. NOTE. |
| ***svID***  This field specifies the satellite for which the data is provided. |
| ***iod***  This field specifies the IOD value of the broadcast ephemeris used for calculation of FKP data (see IE *GNSS‑NavigationModel*). |
| ***north-geometric-gradient***  This field specifies the gradient (FKP) of the geometric (non-dispersive) error components in South-North direction in parts per million of the south-north distance to the reference station.  Scale factor 0.01 ppm; range ±20.47 ppm. |
| ***east-geometric-gradient***  This field specifies the gradient (FKP) of the geometric (non-dispersive) error components in West-East direction in parts per million of the west-east distance to the reference station.  Scale factor 0.01 ppm; range ±20.47 ppm. |
| ***north-ionospheric-gradient***  This field specifies the gradient (FKP) of the ionospheric (dispersive) error component in South-North direction.  Scale factor 0.01 ppm; range ±81.91 ppm. |
| ***east-ionospheric-gradient***  This field specifies the gradient (FKP) of the ionospheric (dispersive) error component in West-East direction.  Scale factor 0.01 ppm; range ±81.91 ppm. |

NOTE: As described in [30], the distance dependent error for the geometric part *0* and ionospheric part *I* is computed from the gradients provided in *FKP-Gradients-Element*. The distance dependent error for a carrier phase measurements *Ф* on a signal with frequency *f* can be computed by:  


where *f1*, *f* is the link/frequency indicated by the *l1*, *l2* fields, respectively.

#### *– GNSS-SSR-OrbitCorrections*

The IE *GNSS-SSR-OrbitCorrections* is used by the location server to provide radial, along-track and cross-track orbit corrections together with integrity information. The target device may use the *SSR-OrbitCorrectionList* to compute a satellite position correction to be combined with the satellite position calculated from broadcast ephemeris.

The parameters provided in IE *GNSS-SSR-OrbitCorrections –* except for *ORBIT-IntegrityParameters* and *SSR-IntegrityOrbitBounds –* are used as specified for SSR Orbit Messages (e.g., message type 1057 and 1063) in [30] and apply to all GNSSs.

-- ASN1START

GNSS-SSR-OrbitCorrections-r15 ::= SEQUENCE {

epochTime-r15 GNSS-SystemTime,

ssrUpdateInterval-r15 INTEGER (0..15),

satelliteReferenceDatum-r15 ENUMERATED { itrf, regional, ... },

iod-ssr-r15 INTEGER (0..15),

ssr-OrbitCorrectionList-r15 SSR-OrbitCorrectionList-r15,

...,

[[

orbit-IntegrityParameters-r17 ORBIT-IntegrityParameters-r17 OPTIONAL -- Need OR

]]

}

SSR-OrbitCorrectionList-r15 ::= SEQUENCE (SIZE(1..64)) OF SSR-OrbitCorrectionSatelliteElement-r15

SSR-OrbitCorrectionSatelliteElement-r15 ::= SEQUENCE {

svID-r15 SV-ID,

iod-r15 BIT STRING (SIZE(11)),

delta-radial-r15 INTEGER (-2097152..2097151),

delta-AlongTrack-r15 INTEGER (-524288..524287),

delta-CrossTrack-r15 INTEGER (-524288..524287),

dot-delta-radial-r15 INTEGER (-1048576..1048575) OPTIONAL, -- Need ON

dot-delta-AlongTrack-r15 INTEGER (-262144..262143) OPTIONAL, -- Need ON

dot-delta-CrossTrack-r15 INTEGER (-262144..262143) OPTIONAL, -- Need ON

...,

[[

ssr-IntegrityOrbitBounds-r17 SSR-IntegrityOrbitBounds-r17 OPTIONAL -- Cond Integrity1

]]

}

ORBIT-IntegrityParameters-r17 ::= SEQUENCE {

probOnsetConstFault-r17 INTEGER (0..255),

meanConstFaultDuration-r17 INTEGER (1..3600),

probOnsetSatFault-r17 INTEGER (0..255),

meanSatFaultDuration-r17 INTEGER (1..3600),

orbitRangeErrorCorrelationTime-r17 INTEGER (0..255) OPTIONAL, -- Need OR

orbitRangeRateErrorCorrelationTime-r17 INTEGER (0..255) OPTIONAL, -- Cond Integrity2

...

}

SSR-IntegrityOrbitBounds-r17 ::= SEQUENCE {

meanOrbitError-r17 RAC-OrbitalErrorComponents-r17,

stdDevOrbitError-r17 RAC-OrbitalErrorComponents-r17,

meanOrbitRateError-r17 RAC-OrbitalErrorComponents-r17,

stdDevOrbitRateError-r17 RAC-OrbitalErrorComponents-r17,

...

}

RAC-OrbitalErrorComponents-r17 ::= SEQUENCE {

radial-r17 INTEGER (0..255),

alongTrack-r17 INTEGER (0..255),

crossTrack-r17 INTEGER (0..255)

}

-- ASN1STOP

| Conditional presence | Explanation |
| --- | --- |
| *Integrity1* | The field is mandatory present if *ORBIT-IntegrityParameters* is present*;* otherwise it is not present. |
| *Integrity2* | The field is mandatory present if *orbitRangeErrorCorrelationTime* is present*;* otherwise it is not present. |

| *GNSS-SSR-OrbitCorrections* field descriptions |
| --- |
| ***epochTime***  This field specifies the epoch time of the orbit corrections. The *gnss-TimeID* in *GNSS-SystemTime* shall be the same as the *GNSS-ID* in IE *GNSS-GenericAssistDataElement*. |
| ***ssrUpdateInterval***  This field specifies the SSR Update Interval. The SSR Update Intervals for all SSR parameters start at time 00:00:00 of the GPS time scale. A change of the SSR Update Interval during the transmission of SSR data should ensure consistent data for a target device. See table Value of *ssrUpdateInterval* to SSR Update Interval relation below. NOTE 1. |
| ***satelliteReferenceDatum***  This field specifies the satellite refence datum for the orbit corrections. |
| ***iod-ssr***  This field specifies the Issue of Data number for the SSR data. A change of *iod-ssr* is used to indicate a change in the SSR generating configuration. |
| ***svID***  This field specifies the satellite for which the orbit corrections are provided. |
| ***iod***  This field specifies the IOD value of the broadcast ephemeris for which the orbit corrections are valid (see IE *GNSS‑NavigationModel*). NOTE 2, NOTE 4. |
| ***delta-radial***  This field specifies the radial orbit correction for broadcast ephemeris. NOTE 3.  Scale factor 0.1 mm; range ±209.7151 m. |
| ***delta-AlongTrack***  This field specifies the along-track orbit correction for broadcast ephemeris. NOTE 3.  Scale factor 0.4 mm; range ±209.7148 m. |
| ***delta-CrossTrack***  This field specifies the cross-track orbit correction for broadcast ephemeris. NOTE 3.  Scale factor 0.4 mm; range ±209.7148 m. |
| ***dot-delta-radial***  This field specifies the velocity of radial orbit correction for broadcast ephemeris. NOTE 3.  Scale factor 0.001 mm/s; range ±1.048575 m/s. |
| ***dot-delta-AlongTrack***  This field specifies the velocity of along-track orbit correction for broadcast ephemeris. NOTE 3.  Scale factor 0.004 mm/s; range ±1.048572 m/s. |
| ***dot-delta-CrossTrack***  This field specifies the velocity of cross-track orbit correction for broadcast ephemeris. NOTE 3.  Scale factor 0.004 mm/s; range ±1.048572 m/s. |
| ***probOnsetConstFault***  This field specifies the Probability of Onset of Constellation Fault per Time Unit where a constellation fault is at least two satellites being faulty simultaneously due to the same event.  This field specifies the onset probability that the residual range or range rate error exceeds a bound created using the minimum allowed inflation factor *Kmin*, and bounding parameters as *mean* + *Kmin* \* *stdDev* where *Kmin* = *normInv*(*irMaximum* / 2), with *irMaximum* as provided in IE *GNSS-Integrity-ServiceParameters*.  The probability is calculated by *P*=10-0.04*n* [hour-1] where *n* is the value of *probOnsetConstFault* and the range is 10-10.2 to 1 per hour. |
| ***meanConstFaultDuration***  This field specifies the Mean Constellation Fault Duration which is the mean duration between when a constellation fault occurs, and the user is alerted by IE *GNSS-RealTimeIntegrity* (or the integrity violation is over).  Scale factor 1 s; range 1-3600 s. |
| ***probOnsetSatFault***  This field specifies the Probability of Onset of Satellite Fault per Time Unit which is the probability of occurrence of satellite error to exceed the residual error bound for more than the Time to Alert (TTA).  This field specifies the onset probability that the residual range or range rate error exceeds a bound created using the minimum allowed inflation factor *Kmin*, and bounding parameters as *mean* + *Kmin* \* *stdDev* where *Kmin* = *normInv*(*irMaximum* / 2), with *irMaximum* as provided in IE *GNSS-Integrity-ServiceParameters*.  The probability is calculated by *P*=10-0.04*n* [hour-1] where *n* is the value of *probOnsetSatFault* and the range is 10-10.2 to 1 per hour. |
| ***meanSatFaultDuration***  This field specifies the Mean Satellite Fault Duration which is the mean duration between when a satellite fault occurs, and the user is alerted by IE *GNSS-RealTimeIntegrity* (or the integrity violation is over).  Scale factor 1 s; range 1-3,600 s. |
| ***orbitRangeErrorCorrelationTime***  This field specifies the Orbit Range Error Correlation Time which is the upper bound of the correlation time of the satellite residual range error due to orbit.  The time is calculated using:  Range is 1-28,200 s. |
| ***orbitRangeRateErrorCorrelationTime***  This field specifies the Orbit Range Rate Error Correlation Time which is the upper bound of the correlation time of the satellite residual range rate error due to orbit.  The time is calculated using:  Range is 1-28,200 s. |
| ***meanOrbitError***  This field specifies the Mean Orbit Error bound in satellite radial, along-track and cross-track coordinates, which are the mean values for a set of three overbounding models that bound the residual orbit error in satellite radial, along-track and cross-track directions.  Each mean is calculated using:  Range is 0-17.5 m. |
| ***stdDevOrbitError***  This field specifies the Standard Deviation Orbit Error bound in satellite radial, along-track and cross-track coordinates, which are the standard deviation values for a set of three overbounding models that bound the residual orbit error in satellite radial, along-track and cross-track directions.  Each standard deviation is calculated using:  Range is 0-17.5 m. |
| ***meanOrbitRateError***  This field specifies the Mean Orbit Rate Error in satellite radial, along-track and cross-track coordinates, which are the mean values for a set of three overbounding models that bound the residual satellite orbit rate error in satellite radial, along-track and cross-track directions.  Scale factor 0.001 m/s; range 0-0.255 m/s. |
| ***stdDevOrbitRateError***  This field specifies the Standard Deviation Orbit Rate Error in satellite radial, along-track and cross-track coordinates, which are the standard deviation values for a set of three overbounding models that bound the residual satellite orbit rate error in satellite radial, along-track and cross-track directions.  Scale factor 0.001 m/s; range 0-0.255 m/s. |

NOTE 1: The update intervals are aligned to the GPS time scale for all GNSSs in order to allow synchronous operation for multiple GNSS services. This means that the update intervals may not be aligned to the beginning of the day for another GNSS. Due to the leap seconds, this is generally the case for GLONASS.

NOTE 2: In the cases that *gnss-ID* indicates 'gps', 'qzss' or 'bds', the *iod* refers to the NAV broadcast ephemeris (GPS L1 C/A, QZSS QZS-L1 or BDS B1I/B3I, respectively, in table GNSS to iod Bit String(11) relation in IE *GNSS‑NavigationModel*).

NOTE 3: The reference time *t0* is *epochTime* + ½ × *ssrUpdateInterval*. The reference time *t0* for *ssrUpdateInterval* '0' is *epochTime*.

NOTE 4: In the cases that the *GNSS-SSR-OrbitCorrection* IE is contained within a *GNSS-SSR-OrbitCorrectionsSet2* IE, then the reference ephemeris is denoted by the *refEph* field within the *GNSS-SSR-OrbitCorrectionsSet2* IE, not the default as per NOTE 2. In the case *gnss-ID* indicates 'bds' and if *refEph* is set to *b1c*, the *iod* refers to the B-CNAV1 broadcast ephemeris (BDS B1C/B2a in table GNSS to iod Bit String (11) relation in IE *GNSS‑NavigationModel*).

Value of *ssrUpdateInterval* to SSR Update Interval relation

|  |  |
| --- | --- |
| Value of *ssrUpdateInterval* | SSR Update Interval |
| 0 | 1 second |
| 1 | 2 seconds |
| 2 | 5 seconds |
| 3 | 10 seconds |
| 4 | 15 seconds |
| 5 | 30 seconds |
| 6 | 60 seconds |
| 7 | 120 seconds |
| 8 | 240 seconds |
| 9 | 300 seconds |
| 10 | 600 seconds |
| 11 | 900 seconds |
| 12 | 1800 seconds |
| 13 | 3600 seconds |
| 14 | 7200 seconds |
| 15 | 10800 seconds |

#### *– GNSS-SSR-ClockCorrections*

The IE *GNSS-SSR-ClockCorrections* is used by the location server to provide clock correction parameters together with integrity information. The target device may use the *SSR-ClockCorrectionList* to compute a clock correction to be applied to the broadcast satellite clock parameters, identified by *iod* of corresponding *GNSS-SSR-OrbitCorrections*.

The parameters provided in IE *GNSS-SSR-ClockCorrections –* except for *CLOCK-IntegrityParameters* and *SSR-IntegrityClockBounds –* are used as specified for SSR Clock Messages (e.g., message type 1058 and 1064) in [30] and apply to all GNSSs.

-- ASN1START

GNSS-SSR-ClockCorrections-r15 ::= SEQUENCE {

epochTime-r15 GNSS-SystemTime,

ssrUpdateInterval-r15 INTEGER (0..15),

iod-ssr-r15 INTEGER (0..15),

ssr-ClockCorrectionList-r15 SSR-ClockCorrectionList-r15,

...,

[[

clock-IntegrityParameters-r17 CLOCK-IntegrityParameters-r17 OPTIONAL -- Need OR

]]

}

SSR-ClockCorrectionList-r15 ::= SEQUENCE (SIZE(1..64)) OF SSR-ClockCorrectionSatelliteElement-r15

SSR-ClockCorrectionSatelliteElement-r15 ::= SEQUENCE {

svID-r15 SV-ID,

delta-Clock-C0-r15 INTEGER (-2097152..2097151),

delta-Clock-C1-r15 INTEGER (-1048576..1048575) OPTIONAL, -- Need ON

delta-Clock-C2-r15 INTEGER (-67108864..67108863) OPTIONAL, -- Need ON

...,

[[

ssr-IntegrityClockBounds-r17 SSR-IntegrityClockBounds-r17 OPTIONAL -- Need OR

]]

}

CLOCK-IntegrityParameters-r17 ::= SEQUENCE {

clockRangeErrorCorrelationTime-r17 INTEGER (0..255),

clockRangeRateErrorCorrelationTime-r17 INTEGER (0..255),

...

}

SSR-IntegrityClockBounds-r17 ::= SEQUENCE {

meanClock-r17 INTEGER (0..255),

stdDevClock-r17 INTEGER (0..255),

meanClockRate-r17 INTEGER (0..255),

stdDevClockRate-r17 INTEGER (0..255),

...

}

-- ASN1STOP

| *GNSS-SSR-ClockCorrections* field descriptions |
| --- |
| ***epochTime***  This field specifies the epoch time of the clock corrections. The gnss-TimeID in *GNSS-SystemTime* shall be the same as the *GNSS-ID* in IE *GNSS-GenericAssistDataElement.* |
| ***ssrUpdateInterval***  This field specifies the SSR Update Interval. The SSR Update Intervals for all SSR parameters start at time 00:00:00 of the GPS time scale. A change of the SSR Update Interval during the transmission of SSR data should ensure consistent data for a target device. See table Value of *ssrUpdateInterval* to SSR Update Interval relation in IE *GNSS‑SSR‑OrbitCorrections*. |
| ***iod-ssr***  This field specifies the Issue of Data number for the SSR data. A change of iod-ssr is used to indicate a change in the SSR generating configuration. |
| ***svID***  This field specifies the satellite for which the clock corrections are provided. |
| ***delta-Clock-C0***  This field specifies the C0 polynomial coefficient for correction of broadcast satellite clock. NOTE 1.  Scale factor 0.1 mm; range ±209.7151 m. |
| ***delta-Clock-C1***  This field specifies the C1 polynomial coefficient for correction of broadcast satellite clock. NOTE 1.  Scale factor 0.001 mm/s; range ±1.048575 m/s. |
| ***delta-Clock-C2***  This field specifies the C2 polynomial coefficient for correction of broadcast satellite clock. NOTE 1.  Scale factor 0.00002 mm/s2; range ±1.34217726 m/s2. |
| ***clockRangeErrorCorrelationTime***  This field specifies the Clock Range Error Correlation Time which is the upper bound of the correlation time of the satellite residual range error due to clock.  The time is calculated using:  Range is 1-28,200 s. |
| ***clockRangeRateErrorCorrelationTime***  This field specifies the Clock Range Rate Error Correlation Time which is the upper bound of the correlation time of the satellite residual range rate error due to clock.  The time is calculated using:  Range is 1-28,200 s. |
| ***meanClock***  This field specifies the Mean Clock Error bound which is the mean value for an overbounding model that bounds the residual clock error.  The bound is *meanClock* + K \* *stdDevClock* and shall be so that the probability of it to be exceeded shall be lower than IRallocation for *irMinimum* < IRallocation < *irMaximum*, where K = normInv(IRallocation / 2) and *irMinimum*, *irMaximum* as provided in IE *GNSS-Integrity-ServiceParameters*.  This IRallocation is a fraction of the Target Integrity Risk that represents the integrity risk budget available.  The mean is calculated using:  Range is 0-17.5 m. |
| ***stdDevClock***  This field specifies the Standard Deviation Clock Error bound which is the standard deviation for an overbounding model that bounds the residual clock error.  The standard deviation is calculated using:  Range is 0-17.5 m. |
| ***meanClockRate***  This field specifies the Mean Clock Rate Error bound which is the mean value for an overbounding model that bounds the residual clock rate error.  The bound is *meanClockRate* + K \* *stdDevClockRate* and shall be so that the probability of it to be exceeded shall be lower than IRallocation for *irMinimum* < IRallocation < *irMaximum*, where K = normInv(IRallocation / 2) and *irMinimum*, *irMaximum* as provided in IE *GNSS-Integrity-ServiceParameters*.  This IRallocation is a fraction of the Target Integrity Risk that represents the integrity risk budget available.  Scale factor 0.001 m/s; range 0.000-0.255 m/s. |
| ***stdDevClockRate***  This field specifies the Standard Deviation Clock Rate Error bound which is the standard deviation for an overbounding model that bounds the residual clock rate error.  Scale factor 0.001 m/s; range 0.000-0.255 m/s. |

NOTE 1: The reference time *t0* is *epochTime* + ½ × *ssrUpdateInterval*. The reference time *t0* for *ssrUpdateInterval* '0' is *epochTime*.

#### *– GNSS-SSR-CodeBias*

The IE *GNSS-SSR-CodeBias* is used by the location server to provide GNSS signal code bias together with integrity information. The target device may add the code bias to the pseudo-range measurement of the corresponding code signal to get corrected pseudo-ranges.

NOTE: Any code biases transmitted in the broadcast messages (e.g., the GPS group delay differential TGD [4] (*NAV‑ClockModel*)) are not applied at all by the target device.

The parameters provided in IE *GNSS-SSR-CodeBias –* except for *SSR-IntegrityCodeBiasBounds –* are used as specified for SSR Code Bias Messages (e.g., message type 1059 and 1065) in [30] and apply to all GNSSs.

-- ASN1START

GNSS-SSR-CodeBias-r15 ::= SEQUENCE {

epochTime-r15 GNSS-SystemTime,

ssrUpdateInterval-r15 INTEGER (0..15),

iod-ssr-r15 INTEGER (0..15),

ssr-CodeBiasSatList-r15 SSR-CodeBiasSatList-r15,

...

}

SSR-CodeBiasSatList-r15 ::= SEQUENCE (SIZE(1..64)) OF SSR-CodeBiasSatElement-r15

SSR-CodeBiasSatElement-r15 ::= SEQUENCE {

svID-r15 SV-ID,

ssr-CodeBiasSignalList-r15 SSR-CodeBiasSignalList-r15,

...

}

SSR-CodeBiasSignalList-r15 ::= SEQUENCE (SIZE(1..16)) OF SSR-CodeBiasSignalElement-r15

SSR-CodeBiasSignalElement-r15 ::= SEQUENCE {

signal-and-tracking-mode-ID-r15 GNSS-SignalID,

codeBias-r15 INTEGER (-8192..8191),

...,

[[

ssr-IntegrityCodeBiasBounds-r17 SSR-IntegrityCodeBiasBounds-r17 OPTIONAL -- Need OR

]]

}

SSR-IntegrityCodeBiasBounds-r17 ::= SEQUENCE {

meanCodeBias-r17 INTEGER (0..255),

stdDevCodeBias-r17 INTEGER (0..255),

meanCodeBiasRate-r17 INTEGER (0..255),

stdDevCodeBiasRate-r17 INTEGER (0..255),

...

}

-- ASN1STOP

| *GNSS-SSR-CodeBias* field descriptions |
| --- |
| ***epochTime***  This field specifies the epoch time of the code bias data. The *gnss-TimeID* in *GNSS-SystemTime* shall be the same as the *GNSS-ID* in IE *GNSS-GenericAssistDataElement*. |
| ***ssrUpdateInterval***  This field specifies the SSR Update Interval. The SSR Update Intervals for all SSR parameters start at time 00:00:00 of the GPS time scale. A change of the SSR Update Interval during the transmission of SSR data should ensure consistent data for a target device. See table Value of *ssrUpdateInterval* to SSR Update Interval relation in IE *GNSS‑SSR‑OrbitCorrections*. |
| ***iod-ssr***  This field specifies the Issue of Data number for the SSR data. A change of *iod-ssr* is used to indicate a change in the SSR generating configuration. |
| ***svID***  This field specifies the GNSS satellite for which the code biases are provided. |
| ***signal-and-tracking-mode-ID***  This field specifies the GNSS signal for which the code biases are provided. |
| ***codeBias***  This field provides the code bias for the GNSS signal indicated by *signal-and-tracking-mode-ID*.  Scale factor 0.01 m; range ±81.91 m. |
| ***meanCodeBias***  This field specifies the Mean Code Bias Error bound which is the mean value for an overbounding model that bounds the residual code bias error.  The bound is *meanCodeBias* + K \* *stdDevCodeBias* and shall be so that the probability of it to be exceeded shall be lower than IRallocation for *irMinimum* < IRallocation < *irMaximum*, where K = normInv(IRallocation / 2) and *irMinimum*, *irMaximum* as provided in IE *GNSS-Integrity-ServiceParameters*.  This IRallocation is a fraction of the Target Integrity Risk that represents the integrity risk budget available.  Scale factor 0.005 m; range 0-1.275 m. |
| ***stdDevCodeBias***  This field specifies the Standard Deviation Code Bias Error bound which is the standard deviation for an overbounding model that bounds the residual code bias error.  Scale factor 0.005 m; range 0-1.275 m. |
| ***meanCodeBiasRate***  This field specifies the Mean Code Bias Rate Error bound which is the mean value for an overbounding model that bounds the residual code bias rate error.  The bound is *meanCodeBiasRate* + K \* *stdDevCodeBiasRate* and shall be so that the probability of it to be exceeded shall be lower than IRallocation for *irMinimum* < IRallocation < *irMaximum*, where K = normInv(IRallocation / 2) and *irMinimum*, *irMaximum* as provided in IE *GNSS-Integrity-ServiceParameters*.  This IRallocation is a fraction of the Target Integrity Risk that represents the integrity risk budget available.  Scale factor 0.00005 m/s; range 0-0.01275 m/s. |
| ***stdDevCodeBiasRate***  This field specifies the Standard Deviation Code Bias Rate Error bound which is the standard deviation for an overbounding model that bounds the residual code bias rate error.  Scale factor 0.00005 m/s; range 0-0.01275 m/s. |

#### *– GNSS-SSR-URA*

The IE *GNSS-SSR-URA* is used by the location server to provide quality information for the provided SSR assistance data.

The parameters provided in IE *GNSS-SSR-URA* are used as specified for the SSR URA Messages (e.g., message type 1061 and 1067) in [30] and apply to all GNSSs.

-- ASN1START

GNSS-SSR-URA-r16 ::= SEQUENCE {

epochTime-r16 GNSS-SystemTime,

ssrUpdateInterval-r16 INTEGER (0..15),

iod-ssr-r16 INTEGER (0..15),

ssr-URA-SatList-r16 SSR-URA-SatList-r16,

...

}

SSR-URA-SatList-r16 ::= SEQUENCE (SIZE(1..64)) OF SSR-URA-SatElement-r16

SSR-URA-SatElement-r16 ::= SEQUENCE {

svID-r16 SV-ID,

ssr-URA-r16 BIT STRING (SIZE (6)),

...

}

-- ASN1STOP

| *GNSS-SSR-URA* field descriptions |
| --- |
| ***epochTime***  This field specifies the epoch time of the SSR User Range Accuracy (URA). The *gnss-TimeID* in *GNSS-SystemTime* shall be the same as the *GNSS-ID* in IE *GNSS-GenericAssistDataElement*. |
| ***ssrUpdateInterval***  This field specifies the SSR Update Interval. The SSR Update Intervals for all SSR parameters start at time 00:00:00 of the GPS time scale. A change of the SSR Update Interval during the transmission of SSR data should ensure consistent data for a target device. See table Value of *ssrUpdateInterval* to SSR Update Interval relation in IE *GNSS‑SSR‑OrbitCorrections*. |
| ***iod-ssr***  This field specifies the Issue of Data number for the SSR data. A change of *iod-ssr* is used to indicate a change in the SSR generating configuration. |
| ***svID***  This field specifies the GNSS satellite for which the SSR URA is provided. |
| ***ssr-URA***  This field specifies the User Range Accuracy (URA) (1-sigma) for the range correction provided in the SSR assistance data. The URA is represented by a combination of CLASS and VALUE. The 3 MSB define the CLASS with a range of 0-7 and the 3 LSB define the VALUE with a range of 0-7. The URA is computed by:  See Table 'Relationship between SSR troposphere quality and URA indicator and physical quantity' in IE *GNSS‑SSR‑GriddedCorrection*. |

#### *– GNSS-SSR-PhaseBias*

The IE *GNSS-SSR-PhaseBias* is used by the location server to provide GNSS signal phase bias together with integrity information. The target device may add the phase bias to the phase-range measurement of the corresponding phase signal to get corrected phase-ranges.

The parameters provided in IE *GNSS-SSR-PhaseBias –* except for *SSR-IntegrityPhaseBiasBounds –* are used as specified for Compact SSR GNSS Satellite Phase Bias Messages (e.g., message type 4073,5) in [43] and apply to all GNSSs.

-- ASN1START

GNSS-SSR-PhaseBias-r16 ::= SEQUENCE {

epochTime-r16 GNSS-SystemTime,

ssrUpdateInterval-r16 INTEGER (0..15),

iod-ssr-r16 INTEGER (0..15),

ssr-PhaseBiasSatList-r16 SSR-PhaseBiasSatList-r16,

...

}

SSR-PhaseBiasSatList-r16 ::= SEQUENCE (SIZE(1..64)) OF SSR-PhaseBiasSatElement-r16

SSR-PhaseBiasSatElement-r16 ::= SEQUENCE {

svID-r16 SV-ID,

ssr-PhaseBiasSignalList-r16 SSR-PhaseBiasSignalList-r16,

...

}

SSR-PhaseBiasSignalList-r16 ::= SEQUENCE (SIZE(1..16)) OF SSR-PhaseBiasSignalElement-r16

SSR-PhaseBiasSignalElement-r16 ::= SEQUENCE {

signal-and-tracking-mode-ID-r16 GNSS-SignalID,

phaseBias-r16 INTEGER (-16384..16383),

phaseDiscontinuityIndicator-r16 INTEGER (0..3),

phaseBiasIntegerIndicator-r16 INTEGER (0..3) OPTIONAL, -- Need OP

...,

[[

ssr-IntegrityPhaseBiasBounds-r17 SSR-IntegrityPhaseBiasBounds-r17 OPTIONAL -- Need OR

]]

}

SSR-IntegrityPhaseBiasBounds-r17 ::= SEQUENCE {

meanPhaseBias-r17 INTEGER (0..255),

stdDevPhaseBias-r17 INTEGER (0..255),

meanPhaseBiasRate-r17 INTEGER (0..255),

stdDevPhaseBiasRate-r17 INTEGER (0..255),

...

}

-- ASN1STOP

| *GNSS-SSR-PhaseBias* field descriptions |
| --- |
| ***epochTime***  This field specifies the epoch time of the phase bias data. The *gnss-TimeID* in *GNSS-SystemTime* shall be the same as the *GNSS-ID* in IE *GNSS-GenericAssistDataElement*. |
| ***ssrUpdateInterval***  This field specifies the SSR Update Interval. The SSR Update Intervals for all SSR parameters start at time 00:00:00 of the GPS time scale. A change of the SSR Update Interval during the transmission of SSR data should ensure consistent data for a target device. See table Value of *ssrUpdateInterval* to SSR Update Interval relation in IE *GNSS‑SSR‑OrbitCorrections*. |
| ***iod-ssr***  This field specifies the Issue of Data number for the SSR data. A change of *iod-ssr* is used to indicate a change in the SSR generating configuration. |
| ***svID***  This field specifies the GNSS satellite for which the phase biases are provided. |
| ***signal-and-tracking-mode-ID***  This field specifies the GNSS signal for which the phase biases are provided. |
| ***phaseBias***  This field provides the phase bias for the GNSS signal indicated by *signal-and-tracking-mode-ID*.  Scale factor 0.001 m; range ±16.383 m. |
| ***phaseDiscontinuityIndicator***  This field provides the phase discontinuity counter for the GNSS signal indicated by *signal-and-tracking-mode-ID*. This counter is increased for every discontinuity in phase (roll-over from 3 to 0). |
| ***phaseBiasIntegerIndicator***  This field informs whether the phase bias is Undifferenced Integer (Value 0), Widelane Integer (Value 1) or Non-Integer (Value 2):  Value 0: The Undifferenced Integer Phase Bias supports PPP-RTK fixed, widelane or float mode.  Value 1: The Widelane Integer Phase Bias indicates that after application of the Phase Bias value, this signal can be differenced with any other signal from the same satellite that also has Widelane Integer Phase Bias indicated to form a new combined carrier phase measurement of integer quality, supporting PPP-RTK widelane fixed mode.  Value 2: The Non-Integer Phase Bias supports PPP-RTK float mode.  Value 3: Reserved.  If the *phaseBiasIntegerIndicator* field is not present then it is interpreted as having Value 0 (Undifferenced Integer). |
| ***meanPhaseBias***  This field specifies the Mean Phase Bias Error bound which is the mean value for an overbounding model that bounds the residual phase bias error.  The bound is *meanPhaseBias* + K \* *stdDevPhaseBias* and shall be so that the probability of it to be exceeded shall be lower than IRallocation for *irMinimum* < IRallocation < *irMaximum*, where K = normInv(IRallocation / 2) and *irMinimum*, *irMaximum* as provided in IE *GNSS-Integrity-ServiceParameters*.  This IRallocation is a fraction of the Target Integrity Risk that represents the integrity risk budget available.  Scale factor 0.005 m; range 0-1.275 m. |
| ***stdDevPhaseBias***  This field specifies the Standard Deviation Phase Bias Error bound which is the standard deviation for an overbounding model that bounds the residual phase bias error.  Scale factor 0.005 m; range 0-1.275 m. |
| ***meanPhaseBiasRate***  This field specifies the Mean Phase Bias Rate Error bound which is the mean value for an overbounding model that bounds the residual phase bias rate error.  The bound is *meanPhaseBiasRate* + K \* *stdDevPhaseBiasRate* and shall be so that the probability of it to be exceeded shall be lower than IRallocation for *irMinimum* < IRallocation < *irMaximum*, where K = normInv(IRallocation / 2) and *irMinimum*, *irMaximum* as provided in IE *GNSS-Integrity-ServiceParameters*.  This IRallocation is a fraction of the Target Integrity Risk that represents the integrity risk budget available.  Scale factor 0.00005 m/s; range 0-0.01275 m/s. |
| ***stdDevPhaseBiasRate***  This field specifies the Standard Deviation Phase Bias Rate Error bound which is the standard deviation for an overbounding model that bounds the residual phase bias rate error.  Scale factor 0.00005 m/s; range 0-0.01275 m/s. |

#### *– GNSS-SSR-STEC-Correction*

The IE *GNSS-SSR-STEC-Correction* is used by the location server to provide ionosphere slant delay correction together with integrity information. The ionosphere slant delay (STEC) consists of the polynomial part provided in *GNSS-SSR-STEC-Correction* and the residual part provided in *GNSS-SSR-GriddedCorrection*.

The parameters provided in IE *GNSS-SSR-STEC-Correction –* except for *STEC-IntegrityParameters* and *STEC-IntegrityErrorBounds –* are used as specified for Compact SSR STEC Correction Messages (e.g., message type 4073,8) in [43] and apply to all GNSSs.

-- ASN1START

GNSS-SSR-STEC-Correction-r16 ::= SEQUENCE {

epochTime-r16 GNSS-SystemTime,

ssrUpdateInterval-r16 INTEGER (0..15),

iod-ssr-r16 INTEGER (0..15),

correctionPointSetID-r16 INTEGER (0..16383),

stec-SatList-r16 STEC-SatList-r16,

...,

[[

stec-IntegrityParameters-r17 STEC-IntegrityParameters-r17 OPTIONAL -- Need OR

]]

}

STEC-SatList-r16 ::= SEQUENCE (SIZE(1..64)) OF STEC-SatElement-r16

STEC-SatElement-r16 ::= SEQUENCE {

svID-r16 SV-ID,

stecQualityIndicator-r16 BIT STRING (SIZE(6)),

stec-C00-r16 INTEGER (-8192..8191),

stec-C01-r16 INTEGER (-2048..2047) OPTIONAL, -- Need ON

stec-C10-r16 INTEGER (-2048..2047) OPTIONAL, -- Need ON

stec-C11-r16 INTEGER (-512..511) OPTIONAL, -- Need ON

...,

[[

stec-IntegrityErrorBounds-r17 STEC-IntegrityErrorBounds-r17 OPTIONAL -- Cond Integrity1

]]

}

STEC-IntegrityParameters-r17 ::= SEQUENCE {

probOnsetIonoFault-r17 INTEGER (0..255),

meanIonoFaultDuration-r17 INTEGER (1..256),

ionoRangeErrorCorrelationTime-r17 INTEGER (1..255) OPTIONAL, -- Need OR

ionoRangeRateErrorCorrelationTime-r17 INTEGER (1..255) OPTIONAL, -- Cond Integrity2

...

}

STEC-IntegrityErrorBounds-r17 ::= SEQUENCE {

meanIonosphere-r17 INTEGER (0..255),

stdDevIonosphere-r17 INTEGER (0..255),

meanIonosphereRate-r17 INTEGER (0..255),

stdDevIonosphereRate-r17 INTEGER (0..255),

...

}

-- ASN1STOP

| Conditional presence | Explanation |
| --- | --- |
| *Integrity1* | The field is mandatory present if *STEC-IntegrityParameters* is present*;* otherwise it is not present. |
| *Integrity2* | The field is mandatory present if *ionoRangeErrorCorrelationTime* is present*;* otherwise it is not present. |

| *GNSS-SSR-STEC-Correction* field descriptions |
| --- |
| ***epochTime***  This field specifies the epoch time of the STEC correction data. The *gnss-TimeID* in *GNSS-SystemTime* shall be the same as the *GNSS-ID* in IE *GNSS-GenericAssistDataElement*. |
| ***ssrUpdateInterval***  This field specifies the SSR Update Interval. The SSR Update Intervals for all SSR parameters start at time 00:00:00 of the GPS time scale. A change of the SSR Update Interval during the transmission of SSR data should ensure consistent data for a target device. See table Value of *ssrUpdateInterval* to SSR Update Interval relation in IE *GNSS‑SSR‑OrbitCorrections*. |
| ***correctionPointSetID***  This field provides the ID of the *GNSS-SSR-CorrectionPoints* set. The reference point used for the STEC calculations (see NOTE below) is the reference pointprovided in IE *GNSS-SSR-CorrectionPoints* with the same *correctionPointSetID.* |
| ***iod-ssr***  This field specifies the Issue of Data number for the SSR data. A change of *iod-ssr* is used to indicate a change in the SSR generating configuration. |
| ***svID***  This field specifies the GNSS satellite for which the STEC corrections are provided. |
| ***stecQualityIndicator***  This field specifies SSR STEC quality indicator. The STEC quality indicator is represented by a combination of CLASS and VALUE. The 3 MSB define the CLASS with a range of 0-7 and the 3 LSB define the VALUE with a range of 0-7. See Table 'Relationship between SSR STEC quality indicator and physical quantity' below. |
| ***stec-C00***  This field provides the polynomial coefficient *C00* used to define the STEC. as defined in [43]. NOTE  Scale factor 0.05 TECU; range ±409.55 TECU. |
| ***stec-C01***  This field provides the polynomial coefficient *C01* used to define the STEC as defined in [43]. NOTE  Scale factor 0.02 TECU/deg; range ±40.94 TECU/deg. |
| ***stec-C10***  This field provides the polynomial coefficient *C10* used to define the STEC as defined in [43]. NOTE  Scale factor 0.02 TECU/deg; range ±40.94 TECU/deg. |
| ***stec-C11***  This field provides the polynomial coefficient *C11* used to define the STEC as defined in [43]. NOTE  Scale factor 0.02 TECU/deg2; range ±10.22 TECU/deg2. |
| ***probOnsetIonoFault***  This field specifies the Probability of Onset of Ionosphere Fault per Time Unit which is the probability of occurrence of ionosphere error to exceed the residual error bound for more than the Time to Alert (TTA).  This field specifies the onset probability that the residual range or range rate error exceeds a bound created using the minimum allowed inflation factor *Kmin*, and bounding parameters as *mean* + *Kmin* \* *stdDev* where *Kmin* = *normInv*(*irMaximum* / 2), with *irMaximum* as provided in IE *GNSS-Integrity-ServiceParameters*.  The probability is calculated by *P*=10-0.04*n* [hour-1] where *n* is the value of *probOnsetIonoFault* and the range is 10-10.2 to 1 per hour. |
| ***meanIonoFaultDuration***  This field specifies the Mean Ionosphere Fault Duration which is the mean duration between when an ionosphere integrity violation occurs, and the user is alerted through *GNSS-Integrity-ServiceAlert* (or the integrity violation is over).  Scale factor 1 s; range 1-256 s. |
| ***ionoRangeErrorCorrelationTime***  This field specifies the Ionosphere Range Error Correlation Time which is the upper bound of the correlation time of the ionosphere residual range error.  The time is calculated using:  Range is 1-28,200 s. |
| ***ionoRangeRateErrorCorrelationTime***  This field specifies the Ionosphere Range Rate Error Correlation Time which is the upper bound of the correlation time of the ionosphere residual range rate error.  The time is calculated using:  Range is 1-28,200 s. |
| ***meanIonosphere***  This field specifies the Mean Ionospherre Error bound which is the mean value for an overbounding model that bounds the residual ionosphere error.  The bound is *meanIonosphere* + *K* \* *stdDevIonosphere* and shall be so that the probability of it to be exceeded shall be lower than IRallocation for *irMinimum* < IRallocation < *irMaximum*, where *K* = normInv(IRallocation / 2) and *irMinimum*, *irMaximum* as provided in IE *GNSS-Integrity-ServiceParameters*.  This IRallocation is a fraction of the Target Integrity Risk that represents the integrity risk budget available.  The mean is calculated using:  Range is 0-17.5 m. |
| ***stdDevIonosphere***  This field specifies the Standard Deviation Ionosphere Error bound which is the standard deviation for an overbounding model that bounds the residual ionosphere error.  The standard deviation is calculated using:  Range is 0-17.5 m. |
| ***meanIonosphereRate***  This field specifies the Mean Ionosphere Rate Error which is the mean value for an overbounding model that bounds the residual ionosphere rate error.  The bound is *meanIonosphereRate* + *K* \* *stdDevIonosphereRate* and shall be so that the probability of it to be exceeded shall be lower than IRallocation for *irMinimum* < IRallocation < *irMaximum*, where *K* = normInv(IRallocation / 2) and *irMinimum*, *irMaximum* as provided in IE *GNSS-Integrity-ServiceParameters*.  This IRallocation is a fraction of the Target Integrity Risk that represents the integrity risk budget available.  Scale factor 0.00005 m/s; range 0-0.01275 m/s. |
| ***stdDevIonosphereRate***  This field specifies the Standard Deviation Ionosphere Rate Error which is the standard deviation for an overbounding model that bounds the residual ionosphere rate error.  Scale factor 0.00005 m/s; range 0-0.01275 m/s. |

NOTE: The polynomial coefficients *C00*, *C01*, *C10*, *C11* are used to define the STEC as follows:

(1) If only *C00* is included in *STEC-SatElement*:

*Iai* = *C00*.

(2) If only *C00, C01* and *C10* are included in *STEC-SatElement*:

*Iai* = *C00 + C01*(* – 0*) *+ C10*(* – 0*).

(3) If all of *C00, C01, C10* and *C11* are included in *STEC-SatElement*:

*Iai* = *C00 + C01*(* – 0*)+ *C10*(* – 0*)*+C11*(* – 0*)(* – 0*).

Other combinations of *C00*, *C01*, *C10*, *C11* than (1)-(3) above are undefined in this version of the specification.

The equations above depend on the latitude ** and longitude ** of an evaluated point and latitude *0* and longitude *0* of the reference point which is defined in IE *GNSS-SSR-CorrectionPoints* (*referencePointLatitude* and *referencePointLongitude*).

Relationship between SSR STEC quality indicator and physical quantity

|  |  |  |  |
| --- | --- | --- | --- |
| CLASS | VALUE | Index | SSR STEC Quality Indicator Q [TECU] |
| 7 | 7 | 63 | 33.6664 < Q |
| 7 | 6 | 62 | 30.2992 < Q ≤ 33.6664 |
| 7 | 5 | 61 | 26.9319 < Q ≤ 30.2992 |
| 7 | 4 | 60 | 23.5647 < Q ≤ 26.9319 |
| 7 | 3 | 59 | 20.1974 < Q ≤ 23.5647 |
| 7 | 2 | 58 | 16.8301 < Q ≤ 20.1974 |
| 7 | 1 | 57 | 13.4629 < Q ≤ 16.8301 |
| 7 | 0 | 56 | 12.3405 < Q ≤ 13.4629 |
| 6 | 7 | 55 | 11.2180 < Q ≤ 12.3405 |
| 6 | 6 | 54 | 10.0956 < Q ≤ 11.2180 |
| 6 | 5 | 53 | 8.9732 < Q ≤ 10.0956 |
| 6 | 4 | 52 | 7.8508 < Q ≤ 8.9732 |
| 6 | 3 | 51 | 6.7284 < Q ≤ 7.8508 |
| 6 | 2 | 50 | 5.6059 < Q ≤ 6.7284 |
| 6 | 1 | 49 | 4.4835 < Q ≤ 5.6059 |
| 6 | 0 | 48 | 4.1094 < Q ≤ 4.4835 |
| 5 | 7 | 47 | 3.7352 < Q ≤ 4.1094 |
| 5 | 6 | 46 | 3.3611 < Q ≤ 3.7352 |
| 5 | 5 | 45 | 2.9870 < Q ≤ 3.3611 |
| 5 | 4 | 44 | 2.6128 < Q ≤ 2.9870 |
| 5 | 3 | 43 | 2.2387 < Q ≤ 2.6128 |
| 5 | 2 | 42 | 1.8645 < Q ≤ 2.2387 |
| 5 | 1 | 41 | 1.4904 < Q ≤ 1.8645 |
| 5 | 0 | 40 | 1.3657 < Q ≤ 1.4904 |
| 4 | 7 | 39 | 1.2410 < Q ≤ 1.3657 |
| 4 | 6 | 38 | 1.1163 < Q ≤ 1.2410 |
| 4 | 5 | 37 | 0.9915 < Q ≤ 1.1163 |
| 4 | 4 | 36 | 0.8668 < Q ≤ 0.9915 |
| 4 | 3 | 35 | 0.7421 < Q ≤ 0.8668 |
| 4 | 2 | 34 | 0.6174 < Q ≤ 0.7421 |
| 4 | 1 | 33 | 0.4927 < Q ≤ 0.6174 |
| 4 | 0 | 32 | 0.4511 < Q ≤ 0.4927 |
| 3 | 7 | 31 | 0.4096 < Q ≤ 0.4511 |
| 3 | 6 | 30 | 0.3680 < Q ≤ 0.4096 |
| 3 | 5 | 29 | 0.3264 < Q ≤ 0.3680 |
| 3 | 4 | 28 | 0.2848 < Q ≤ 0.3264 |
| 3 | 3 | 27 | 0.2433 < Q ≤ 0.2848 |
| 3 | 2 | 26 | 0.2017 < Q ≤ 0.2433 |
| 3 | 1 | 25 | 0.1601 < Q ≤ 0.2017 |
| 3 | 0 | 24 | 0.1463 < Q ≤ 0.1601 |
| 2 | 7 | 23 | 0.1324 < Q ≤ 0.1463 |
| 2 | 6 | 22 | 0.1186 < Q ≤ 0.1324 |
| 2 | 5 | 21 | 0.1047 < Q ≤ 0.1186 |
| 2 | 4 | 20 | 0.0908 < Q ≤ 0.1047 |
| 2 | 3 | 19 | 0.0770 < Q ≤ 0.0908 |
| 2 | 2 | 18 | 0.0631 < Q ≤ 0.0770 |
| 2 | 1 | 17 | 0.0493 < Q ≤ 0.0631 |
| 2 | 0 | 16 | 0.0447 < Q ≤ 0.0493 |
| 1 | 7 | 15 | 0.0400 < Q ≤ 0.0447 |
| 1 | 6 | 14 | 0.0354 < Q ≤ 0.0400 |
| 1 | 5 | 13 | 0.0308 < Q ≤ 0.0354 |
| 1 | 4 | 12 | 0.0262 < Q ≤ 0.0308 |
| 1 | 3 | 11 | 0.0216 < Q ≤ 0.0262 |
| 1 | 2 | 10 | 0.0169 < Q ≤ 0.0216 |
| 1 | 1 | 9 | 0.0123 < Q ≤ 0.0169 |
| 1 | 0 | 8 | 0.0108 < Q ≤ 0.0123 |
| 0 | 7 | 7 | 0.0092 < Q ≤ 0.0108 |
| 0 | 6 | 6 | 0.0077 < Q ≤ 0.0092 |
| 0 | 5 | 5 | 0.0062 < Q ≤ 0.0077 |
| 0 | 4 | 4 | 0.0046 < Q ≤ 0.0062 |
| 0 | 3 | 3 | 0.0031 < Q ≤ 0.0046 |
| 0 | 2 | 2 | 0.0015 < Q ≤ 0.0031 |
| 0 | 1 | 1 | Q ≤ 0.0015 |
| 0 | 0 | 0 | undefined/unknown |

#### *– GNSS-SSR-GriddedCorrection*

The IE *GNSS-SSR-GriddedCorrection* is used by the location server to provide troposphere delay correction, together with the residual part of the STEC corrections and integrity information.

The parameters provided in IE *GNSS-SSR-GriddedCorrection* *–* except for *SSR-GriddedCorrectionIntegrityParameters* and *TropoDelayIntegrityErrorBounds –* are used as specified for Compact SSR Gridded Correction Message (e.g., message type 4073,9) in [43] and apply to all GNSSs.

-- ASN1START

GNSS-SSR-GriddedCorrection-r16 ::= SEQUENCE {

epochTime-r16 GNSS-SystemTime,

ssrUpdateInterval-r16 INTEGER (0..15),

iod-ssr-r16 INTEGER (0..15),

troposphericDelayQualityIndicator-r16 BIT STRING (SIZE(6)) OPTIONAL, -- Cond Tropo

correctionPointSetID-r16 INTEGER (0..16383),

gridList-r16 GridList-r16,

...,

[[

ssr-GriddedCorrectionIntegrityParameters-r17

SSR-GriddedCorrectionIntegrityParameters-r17

OPTIONAL -- Need OR

]]

}

GridList-r16 ::= SEQUENCE (SIZE(1..64)) OF GridElement-r16

GridElement-r16 ::= SEQUENCE {

tropospericDelayCorrection-r16 TropospericDelayCorrection-r16 OPTIONAL, -- Need ON

stec-ResidualSatList-r16 STEC-ResidualSatList-r16 OPTIONAL, -- Need ON

...

}

TropospericDelayCorrection-r16 ::= SEQUENCE {

tropoHydroStaticVerticalDelay-r16 INTEGER (-256..255),

tropoWetVerticalDelay-r16 INTEGER (-128..127),

...,

[[

tropoDelayIntegrityErrorBounds-r17 TropoDelayIntegrityErrorBounds-r17

OPTIONAL -- Cond Integrity1

]]

}

STEC-ResidualSatList-r16 ::= SEQUENCE (SIZE(1..64)) OF STEC-ResidualSatElement-r16

STEC-ResidualSatElement-r16 ::= SEQUENCE {

svID-r16 SV-ID,

stecResidualCorrection-r16 CHOICE {

b7-r16 INTEGER (-64..63),

b16-r16 INTEGER (-32768..32767)

},

...

}

SSR-GriddedCorrectionIntegrityParameters-r17 ::= SEQUENCE {

probOnsetTroposphereFault-r17 INTEGER (0..255),

meanTroposphereFaultDuration-r17 INTEGER (1..256),

troposphereRangeErrorCorrelationTime-r17 INTEGER (1..255) OPTIONAL, -- Need OR

troposphereRangeRateErrorCorrelationTime-r17 INTEGER (1..255) OPTIONAL, -- Cond Integrity2

...

}

TropoDelayIntegrityErrorBounds-r17 ::= SEQUENCE {

meanTroposphereVerticalHydroStaticDelay-r17 INTEGER (0..255),

stdDevTroposphereVerticalHydroStaticDelay-r17 INTEGER (0..255),

meanTroposphereVerticalWetDelay-r17 INTEGER (0..255),

stdDevTroposphereVerticalWetDelay-r17 INTEGER (0..255),

meanTroposphereVerticalHydroStaticDelayRate-r17 INTEGER (0..255),

stdDevTroposphereVerticalHydroStaticDelayRate-r17 INTEGER (0..255),

meanTroposphereVerticalWetDelayRate-r17 INTEGER (0..255),

stdDevTroposphereVerticalWetDelayRate-r17 INTEGER (0..255),

...

}

-- ASN1STOP

| Conditional presence | Explanation |
| --- | --- |
| *Tropo* | The field is mandatory present if *tropospericDelayCorrection* is included in *gridList*. Otherwise it is not present. |
| *Integrity1* | The field is mandatory present if *SSR-GriddedCorrectionIntegrityParameters* is present; otherwise it is not present. |
| *Integrity2* | The field is mandatory present if *troposphereRangeErrorCorrelationTime* is present; otherwise it is not present. |

| *GNSS-SSR-GriddedCorrection* field descriptions |
| --- |
| ***epochTime***  This field specifies the epoch time of the gridded correction data. The *gnss-TimeID* in *GNSS-SystemTime* shall be the same as the *GNSS-ID* in IE *GNSS-GenericAssistDataElement*. |
| ***ssrUpdateInterval***  This field specifies the SSR Update Interval. The SSR Update Intervals for all SSR parameters start at time 00:00:00 of the GPS time scale. A change of the SSR Update Interval during the transmission of SSR data should ensure consistent data for a target device. See table Value of *ssrUpdateInterval* to SSR Update Interval relation in IE *GNSS‑SSR‑OrbitCorrections*. |
| ***iod-ssr***  This field specifies the Issue of Data number for the SSR data. A change of *iod-ssr* is used to indicate a change in the SSR generating configuration. |
| ***troposphericDelayQualityIndicator***  This field specifies the quality indicator of the tropospheric delay. The troposphere quality indicator is represented by a combination of CLASS and VALUE. The 3 MSB define the CLASS with a range of 0-7 and the 3 LSB define the VALUE with a range of 0-7. The troposphere quality indicator is computed by:  See Table 'Relationship between SSR troposphere quality and URA indicator and physical quantity' below. |
| ***correctionPointSetID***  This field provides the ID of the *GNSS-SSR-CorrectionPoints* set. The *GNSS-SSR-GriddedCorrection* are valid for the correction points provided in IE *GNSS-SSR-CorrectionPoints* with the same *correctionPointSetID.* |
| ***gridList***  This field provides the troposphere delay correction together with the residual part of the STEC corrections for up to 64 correction points defined in IE *GNSS-SSR-CorrectionPoints*.  If the IE *GNSS-SSR-CorrectionPoints,* which belongs to the *correctionPointSetID*, includes the *listOfCorrectionPoints*, the *gridList* includes the same number of entries, and listed in the same order, as in the *listOfCorrectionPoints.*  If the IE *GNSS-SSR-CorrectionPoints,* which belongs to this *correctionPointSetID*, includes the *arrayOfCorrectionPoints* the *gridList* includes the same number of entries, and listed in the same order, as defined by the enabled bits in the *bitmaskOfGrids*. |
| ***tropoHydroStaticVerticalDelay***  This field specifies the variation in the hydro static troposphere vertical delay relative to nominal value. The target device should add the constant nominal value of 2.3 m to calculate the tropospheric hydro-static vertical delay.  Scale factor 0.004 m; range ±1.02 m. |
| ***tropoWetVerticalDelay***  This field specifies the variation in the wet troposphere vertical delay relative to nominal value. The target device should add the constant value of 0.252 m to calculate the tropospheric wet (non hydro-static) vertical delay.  Scale factor 0.004 m; range ±0.508 m. |
| ***svID***  This field specifies the GNSS satellite for which the STEC residual corrections are provided. |
| ***stecResidualCorrection***  This field specifies the STEC residual correction.  Scale factor 0.04 TECU; range ±2.52 TECU (b7) or ±1310.68 TECU (b16). |
| ***probOnsetTroposphereFault***  This field specifies the Probability of Onset of Troposphere Fault per Time Unit which is the probability of occurrence of troposphere error to exceed the residual error bound for more than the Time to Alert (TTA) This field specifies the onset probability that the residual range or range rate error exceeds a bound created using the minimum allowed inflation factor *Kmin*, and bounding parameters as *mean* + *Kmin* \* *stdDev* where *Kmin* = normInv(*irMaximum* / 2) and *irMaximum* as provided in IE *GNSS-Integrity-ServiceParameters*.  The probability is calculated by P=10-0.04n [hour-1] where *n* is the value of *probOnsetTroposphereFault* and the range is 10-10.2 to 1 per hour. |
| ***meanTroposphereFaultDuration***  This field specifies the Mean Troposphere Fault Duration which is the mean duration between when a troposphere integrity violation occurs, and the user is alerted through *GNSS-Integrity-ServiceAlert* (or the integrity violation is over).  Scale factor 1 s; range 1-256 s. |
| ***troposphereRangeErrorCorrelationTime***  This field specifies the Troposphere Range Error Correlation Time which is the upper bound of the correlation time of the troposphere residual range error.  The time is calculated using:  Range is 1-28,200 s. |
| ***troposphereRangeRateErrorCorrelationTime***  This field specifies the Troposphere Range Rate Error Correlation Time which is the upper bound of the correlation time of the troposphere residual range rate error.  The time is calculated using:  Range is 1-28,200 s. |
| ***meanTroposphereVerticalHydroStaticDelay***  This field specifies the Mean Troposphere Vertical Hydro Static Delay Error bound which is the mean value for an overbounding model that bounds the residual troposphere error in the vertical hydro static delay component.  The bound is *meanTroposphereVerticalHydroStaticDelay* + K \* *stdDevTroposphereVerticalHydroStaticDelay* and shall be so that the probability of it to be exceeded shall be lower than IRallocation for *irMinimum* < IRallocation < *irMaximum*, where K = normInv(IRallocation / 2) and *irMinimum*, *irMaximum* as provided in IE *GNSS-Integrity-ServiceParameters*.  This IRallocation is a fraction of the Target Integrity Risk that represents the integrity risk budget available.  Scale factor 0.005 m; range 0-1.275 m. |
| ***stdDevTroposphereVerticalHydroStaticDelay***  This field specifies the Standard Deviation Troposphere Vertical Hydro Static Delay Error bound which is the standard deviation for an overbounding model that bounds the residual troposphere error in the vertical hydro static delay component.  Scale factor 0.005 m; range 0-1.275 m. |
| ***meanTroposphereVerticalWetDelay***  This field specifies the Mean Troposphere Vertical Wet Static Delay Error bound which is the mean value for an overbounding model that bounds the residual troposphere error in the vertical wet delay component.  The bound is *meanTroposphereVerticalWetDelay* + K \* *stdDevTroposphereVerticalWetDelay* and shall be so that the probability of it to be exceeded shall be lower than IRallocation for *irMinimum* < IRallocation < *irMaximum*, where K = normInv(IRallocation / 2) and *irMinimum*, *irMaximum* as provided in IE *GNSS-Integrity-ServiceParameters*.  This IRallocation is a fraction of the Target Integrity Risk that represents the integrity risk budget available.  Scale factor 0.005 m; range 0-1.275 m. |
| ***stdDevTroposphereVerticalWetDelay***  This field specifies the Standard Deviation Troposphere Vertical Wet Static Delay Error bound which is the standard deviation for an overbounding model that bounds the residual troposphere error in the vertical wet delay component.  Scale factor 0.005 m; range 0-1.275 m. |
| ***meanTroposphereVerticalHydroStaticDelayRate***  This field specifies the Mean Troposphere Vertical Hydro Static Delay Rate Error bound which is the mean value for an overbounding model that bounds the residual troposphere rate error in the vertical hydro static delay component.  The bound is *meanTroposphereVerticalHydroStaticDelayRate* + K \* *stdDevTroposphereVerticalHydroStaticDelayRate* and shall be so that the probability of it to be exceeded shall be lower than IRallocation for *irMinimum* < IRallocation < *irMaximum*, where K = normInv(IRallocation / 2) and *irMinimum*, *irMaximum* as provided in IE *GNSS-Integrity-ServiceParameters*.  This IRallocation is a fraction of the Target Integrity Risk that represents the integrity risk budget available.  Scale factor 0.00005 m/s; range 0-0.01275 m/s. |
| ***stdDevTroposphereVerticalHydroStaticDelayRate***  This field specifies the Standard Deviation Troposphere Vertical Hydro Static Delay Rate Error bound which is the standard deviation for an overbounding model that bounds the residual troposphere rate error in the vertical hydro static delay component.  Scale factor 0.00005 m/s; range 0-0.01275 m/s. |
| ***meanTroposphereVerticalWetDelayRate***  This field specifies the Mean Troposphere Vertical Wet Static Delay Rate Error bound which is the mean value for an overbounding model that bounds the residual troposphere rate error in the vertical wet delay component.  The bound is *meanTroposphereVerticalWetDelayRate* + K \* *stdDevTroposphereVerticalWetDelayRate* and shall be so that the probability of it to be exceeded shall be lower than IRallocation for *irMinimum* < IRallocation < *irMaximum*, where K = normInv(IRallocation / 2) and *irMinimum*, *irMaximum* as provided in IE *GNSS-Integrity-ServiceParameters*.  This IRallocation is a fraction of the Target Integrity Risk that represents the integrity risk budget available.  Scale factor 0.00005 m/s; range 0-0.01275 m/s. |
| ***stdDevTroposphereVerticalWetDelayRate***  This field specifies the Standard Deviation Troposphere Vertical Wet Static Delay Rate Error bound which is the standard deviation for an overbounding model that bounds the residual troposphere rate error in the vertical wet delay component.  Scale factor 0.00005 m/s; range 0-0.01275 m/s. |

Relationship between SSR troposphere quality and URA indicator and physical quantity

|  |  |  |  |
| --- | --- | --- | --- |
| CLASS | VALUE | Index | SSR troposphere quality indicator  and  SSR URA  Q [mm] |
| 7 | 7 | 63 | 5466.50 < Q |
| 7 | 6 | 62 | 4919.75 < Q ≤ 5466.50 |
| 7 | 5 | 61 | 4373.75 < Q ≤ 4919.75 |
| 7 | 4 | 60 | 3826.25 < Q ≤ 4373.00 |
| 7 | 3 | 59 | 3279.50 < Q ≤ 3826.25 |
| 7 | 2 | 58 | 2732.75 < Q ≤ 3279.50 |
| 7 | 1 | 57 | 2186.00 < Q ≤ 2732.75 |
| 7 | 0 | 56 | 2003.75 < Q ≤ 2186.00 |
| 6 | 7 | 55 | 1821.50 < Q ≤ 2003.75 |
| 6 | 6 | 54 | 1639.25 < Q ≤ 1821.50 |
| 6 | 5 | 53 | 1457.00 < Q ≤ 1639.25 |
| 6 | 4 | 52 | 1274.75 < Q ≤ 1457.00 |
| 6 | 3 | 51 | 1092.50 < Q ≤ 1274.75 |
| 6 | 2 | 50 | 910.25 < Q ≤ 1092.50 |
| 6 | 1 | 49 | 728.00 < Q ≤ 910.25 |
| 6 | 0 | 48 | 667.25 < Q ≤ 728.00 |
| 5 | 7 | 47 | 606.50 < Q ≤ 667.25 |
| 5 | 6 | 46 | 545.75 < Q ≤ 606.50 |
| 5 | 5 | 45 | 485.00 < Q ≤ 545.75 |
| 5 | 4 | 44 | 424.25 < Q ≤ 485.00 |
| 5 | 3 | 43 | 363.50 < Q ≤ 425.25 |
| 5 | 2 | 42 | 302.75 < Q ≤ 363.50 |
| 5 | 1 | 41 | 242.00 < Q ≤ 302.75 |
| 5 | 0 | 40 | 221.75 < Q ≤ 242.00 |
| 4 | 7 | 39 | 201.50 < Q ≤ 221.75 |
| 4 | 6 | 38 | 181.25 < Q ≤ 201.50 |
| 4 | 5 | 37 | 161.00 < Q ≤ 181.25 |
| 4 | 4 | 36 | 140.75 < Q ≤ 161.00 |
| 4 | 3 | 35 | 120.50 < Q ≤ 140.75 |
| 4 | 2 | 34 | 100.25 < Q ≤ 120.50 |
| 4 | 1 | 33 | 80.00 < Q ≤ 100.25 |
| 4 | 0 | 32 | 73.25 < Q ≤ 80.00 |
| 3 | 7 | 31 | 66.50 < Q ≤ 73.25 |
| 3 | 6 | 30 | 59.75 < Q ≤ 66.50 |
| 3 | 5 | 29 | 53.00 < Q ≤ 59.75 |
| 3 | 4 | 28 | 46.25 < Q ≤ 53.00 |
| 3 | 3 | 27 | 39.50 < Q ≤ 46.25 |
| 3 | 2 | 26 | 32.75 < Q ≤ 39.50 |
| 3 | 1 | 25 | 26.00 < Q ≤ 32.75 |
| 3 | 0 | 24 | 23.75 < Q ≤ 26.00 |
| 2 | 7 | 23 | 21.50 < Q ≤ 23.75 |
| 2 | 6 | 22 | 19.25 < Q ≤ 21.50 |
| 2 | 5 | 21 | 17.00 < Q ≤ 19.25 |
| 2 | 4 | 20 | 14.75 < Q ≤ 17.00 |
| 2 | 3 | 19 | 12.50 < Q ≤ 14.75 |
| 2 | 2 | 18 | 10.25 < Q ≤ 12.50 |
| 2 | 1 | 17 | 8.00 < Q ≤ 10.25 |
| 2 | 0 | 16 | 7.25 < Q ≤ 8.00 |
| 1 | 7 | 15 | 6.50 < Q ≤ 7.25 |
| 1 | 6 | 14 | 5.75 < Q ≤ 6.50 |
| 1 | 5 | 13 | 5.00 < Q ≤ 5.75 |
| 1 | 4 | 12 | 4.25 < Q ≤ 5.00 |
| 1 | 3 | 11 | 3.50 < Q ≤ 4.25 |
| 1 | 2 | 10 | 2.75 < Q ≤ 3.50 |
| 1 | 1 | 9 | 2.00 < Q ≤ 2.75 |
| 1 | 0 | 8 | 1.75 < Q ≤ 2.00 |
| 0 | 7 | 7 | 1.50 < Q ≤ 1.75 |
| 0 | 6 | 6 | 1.25 < Q ≤ 1.50 |
| 0 | 5 | 5 | 1.00 < Q ≤ 1.25 |
| 0 | 4 | 4 | 0.75 < Q ≤ 1.00 |
| 0 | 3 | 3 | 0.50 < Q ≤ 0.75 |
| 0 | 2 | 2 | 0.25 < Q ≤ 0.50 |
| 0 | 1 | 1 | Q ≤ 0.25 |
| 0 | 0 | 0 | undefined/unknown |

#### – *NavIC-DifferentialCorrections*

The IE *NavIC-DifferentialCorrections* parameters provide users with sets of correction terms that apply to the clock and ephemeris data transmitted by other satellites in the AutoNav mode as defined in [38] under clause 6.2.6.

-- ASN1START

NavIC-DifferentialCorrections-r16 ::= SEQUENCE {

navic-RefTOWC-r16 INTEGER (0..50400),

navic-CorrectionListAutoNav-r16 NavIC-CorrectionListAutoNav-r16,

...

}

NavIC-CorrectionListAutoNav-r16 ::= SEQUENCE (SIZE (1..64)) OF NavIC-CorrectionElementAutoNav-r16

NavIC-CorrectionElementAutoNav-r16 ::= SEQUENCE {

svID SV-ID,

navic-Tod-r16 INTEGER (0..65535),

navic-iodec-r16 INTEGER (0..255),

navic-UDRAI-r16 INTEGER (-16..15),

navic-UDRArateI-r16 INTEGER (-16..15),

navic-EDC-r16 NavIC-EDC-r16,

navic-CDC-r16 NavIC-CDC-r16,

...

}

NavIC-EDC-r16 ::= SEQUENCE {

navic-AlphaEDC-r16 INTEGER (-8192..8191),

navic-BetaEDC-r16 INTEGER (-8192..8191),

navic-GammaEDC-r16 INTEGER (-16384..16383),

navic-AoIcorrection-r16 INTEGER (-2048..2047),

navic-AoRAcorrection-r16 INTEGER (-2048..2047),

navic-SemiMajorcorrection-r16 INTEGER (-2048..2047),

...

}

NavIC-CDC-r16 ::= SEQUENCE {

navic-ClockBiasCorrection-r16 INTEGER (-4096..4095),

navic-ClockDriftCorrection-r16 INTEGER (-128..127),

...

}

-- ASN1STOP

| *NavIC-DifferentialCorrections* field descriptions |
| --- |
| ***navic-RefTOWC***  The transmission timing of the navigation message provided through the Time of Week Count (TOWC) corresponding to the given set of grid ionospheric parameters. It indicates the number of 12 second counts represented in 17 bits. The TOW count value ranges from 1 to 50400 to cover one entire week. The Time of Week (TOW) in seconds is obtained by multiplying TOWC with 12 as defined in [38], clause 5.7. |
| ***navic-Tod***  This field indicates the NavIC Time of Differential Correction in seconds.  Scale factor 16 seconds |
| ***navic-iodec***  This field indicates Issue of Data Ephemeris and Clock which provides the user with a convenient means of detecting any change in the ephemeris and clock parameters as described under clause 6.2.1.3 in [38] |
| ***navic-UDRAI***  This field indicates the index for the User Differential Range Accuracy (in metres) value which enables users to estimate the accuracy obtained after differential corrections are applied as described under clause 6.2.6 in [38] |
| ***navic-UDRArateI***  This field indicates the index for the change rate of User Differential Range Accuracy (metres/second)value which enables users to estimate the accuracy obtained after differential corrections are applied as described under clause 6.2.6 in [38] |
| ***navic-AlphaEDC***  This field indicates the Alpha correction to Ephemeris parameter (Δα), which is one of the six keplerian elements defining the ephemeris differential corrections (EDC) for NavIC as defined under clause 6.1.3.5 in [38].  Scale factor 2–34 |
| ***navic-BetaEDC***  This field indicates Beta correction to Ephemeris parameter (Δβ), which is one of the six keplerian elements defining the ephemeris differential corrections (EDC) for NavIC as defined under clause 6.1.3.5 in [38].  Scale factor 2–34 |
| ***navic-GammaEDC***  This field indicates the Gamma correction to Ephemeris parameter (Δγ), which is one of the six keplerian elements defining the ephemeris differential corrections (EDC) for NavIC as defined under clause 6.1.3.5 in [38].  Scale factor 2–32 semi-circles. |
| ***navic-AoIcorrection***  This field indicates the Angle of inclination correction (Δi), which is one of the six keplerian elements defining the ephemeris differential corrections (EDC) for NavIC as defined under clause 6.1.3.5 in [38].  Scale factor 2–32 semi-circles. |
| ***navic-AoRAcorrection***  This field indicates the Angle of right ascension correction (ΔΩ), which is one of the six keplerian elements defining the ephemeris differential corrections (EDC) for NavIC as defined under clause 6.1.3.5 in [38].  Scale factor 2–32 semi-circles. |
| ***navic-SemiMajorcorrection***  This field indicates the Semi-major correction (ΔA), which is one of the six keplerian elements defining the ephemeris differential corrections (EDC) for NavIC as defined under clause 6.1.3.5 in [38].  Scale factor 2–9 metres. |
| ***navic-ClockBiasCorrection***  This field indicates correction to the satellite clock bias coefficient (δaf0), which is one of the two Satellite clock differential corrections (CDC) containing corrections to the NavIC satellite clock polynomial coefficients as defined under clause 6.1.3.5 in [38].  Scale factor 2–35 seconds. |
| ***navic-ClockDriftCorrection***  This field indicates correction to the satellite clock drift coefficient (δaf1), which is one of the two Satellite clock differential corrections (CDC) containing corrections to the NavIC satellite clock polynomial coefficients as defined under clause 6.1.3.5 in [38].  Scale factor 2–51 sec / sec. |

#### – *NavIC-GridModelParameter*

-- ASN1START

NavIC-GridModelParameter-r16 ::= SEQUENCE {

navic-RefTOWC-r16 INTEGER (0..50400),

regionMasked-r16 INTEGER (0..1023),

regionIgpList-r16 RegionIgpList-r16,

...

}

RegionIgpList-r16 ::= SEQUENCE (SIZE (1..16)) OF RegionIgpElement-r16

RegionIgpElement-r16 ::= SEQUENCE {

regionID-r16 INTEGER (0..15),

givei1-r16 INTEGER (0..15),

givd1-r16 INTEGER (0..511),

givei2-r16 INTEGER (0..15),

givd2-r16 INTEGER (0..511),

givei3-r16 INTEGER (0..15),

givd3-r16 INTEGER (0..511),

givei4-r16 INTEGER (0..15),

givd4-r16 INTEGER (0..511),

givei5-r16 INTEGER (0..15),

givd5-r16 INTEGER (0..511),

givei6-r16 INTEGER (0..15),

givd6-r16 INTEGER (0..511),

givei7-r16 INTEGER (0..15),

givd7-r16 INTEGER (0..511),

givei8-r16 INTEGER (0..15),

givd8-r16 INTEGER (0..511),

givei9-r16 INTEGER (0..15),

givd9-r16 INTEGER (0..511),

givei10-r16 INTEGER (0..15),

givd10-r16 INTEGER (0..511),

givei11-r16 INTEGER (0..15),

givd11-r16 INTEGER (0..511),

givei12-r16 INTEGER (0..15),

givd12-r16 INTEGER (0..511),

givei13-r16 INTEGER (0..15),

givd13-r16 INTEGER (0..511),

givei14-r16 INTEGER (0..15),

givd14-r16 INTEGER (0..511),

givei15-r16 INTEGER (0..15),

givd15-r16 INTEGER (0..511),

...

}

-- ASN1STOP

| *NavIC-GridModelParameter* field descriptions |
| --- |
| ***navic-RefTOWC***  The transmission timing of the navigation message provided through the Time of Week Count (TOWC) corresponding to the given set of grid ionospheric parameters. It indicates the number of 12 second counts represented in 17 bits. The TOW count value ranges from 1 to 50400 to cover one entire week. The Time of Week (TOW) in seconds is obtained by multiplying TOWC with 12 as defined in [38], clause 5.7. |
| ***regionMasked***  Total 90 Ionospheric Grid Points(IGP) are defined in [38] clause 6.2.3 table 25. 15 IGP points are grouped into a single region. The region masked indicates the total number of regions for which the corrections are provided. For the current service area of the IRNSS, regions masked are 6. |
| ***regionIgpList***  This list provides the set of IGPs corresponding to each region. Up to 6 instances (0 to 5) are used in this version of the specification. The values 6 to 15 are reserved for future use. |
| ***regionID***  regionID along with index of the IGPS point corresponding gives the location of IGPS point as defined in [38], table 25, clause 6.2.3. |
| ***givei1, give2, .. , give15***  This field indicates the Grid Ionospheric Vertical Error Index (GIVEI) which is used to describe the delay correction accuracy at ionospheric grid point indicated by the *igp-ID*, the mapping between GIVEI and GIVE is defined in [38], clause 6.2.2 and table 27. |
| ***givd1, givd2, … , givd15***  This field indicates the Grid Ionospheric Vertical Delay (GIVD) as defined in [38], clause 5.3.3.8.1, i.e. the vertical delay at the corresponding Ionospheric Grid points (IGPs) indicated by *igp-ID*. The scale factor is 0.125 metre. |

#### *– GNSS-SSR-OrbitCorrectionsSet2*

The IE *GNSS-SSR-OrbitCorrectionsSet2* is used by the location server to provide SSR orbit correction parameters in the cases where a reference ephemeris is used other than the default ephemeris type used in *GNSS-SSR-OrbitCorrections*.

-- ASN1START

GNSS-SSR-OrbitCorrectionsSet2-r17 ::= SEQUENCE {

refEph-r17 ENUMERATED { b1c,...},

gnss-SSR-OrbitCorrections-r17 GNSS-SSR-OrbitCorrections-r15,

...

}

-- ASN1STOP

| *GNSS-SSR-OrbitCorrectionsSet2* field descriptions |
| --- |
| ***refEph***  This field specifies the reference ephemeris that the SSR orbit corrections refer to. In the case that *gnss-ID* indicates 'bds' and *refEph* indicates b1c, the SSR orbit corrections are referenced to BDS B1C/B2a in table GNSS to iod Bit String (11) relation in IE GNSS‑NavigationModel (i.e. the B-CNAV1 broadcast ephemeris [52]). |
| ***gnss-SSR-OrbitCorrections***  This field specifies the orbit correction parameters which refer to the reference ephemeris indicated by *refEph*. |

#### – *GNSS-SSR-ClockCorrectionsSet2*

The IE *GNSS-SSR-ClockCorrectionsSet2* is used by the location server to provide SSR clock correction parameters in the cases where a reference ephemeris is used other than the default ephemeris type used in *GNSS-SSR-ClockCorrections*.

-- ASN1START

GNSS-SSR-ClockCorrectionsSet2-r17 ::= SEQUENCE {

refEph-r17 ENUMERATED { b1c,...},

gnss-SSR-ClockCorrections-r17 GNSS-SSR-ClockCorrections-r15,

...

}

-- ASN1STOP

| *GNSS-SSR-ClockCorrectionsSet2* field descriptions |
| --- |
| ***refEph***  This field specifies the reference ephemeris that the SSR clock corrections refer to. In the case that *gnss-ID* indicates 'bds' and *refEph* indicates b1c, the SSR clock corrections are referenced to BDS B1C/B2a in table GNSS to iod Bit String (11) relation in IE GNSS‑NavigationModel (i.e. the B-CNAV1 broadcast ephemeris [52]). |
| ***gnss-SSR-ClockCorrections***  This field specifies the clock correction parameters which refer to the reference ephemeris indicated by *refEph*. |

#### – *GNSS-SSR-URA-Set2*

The IE *GNSS-SSR-URA-Set2* is used by the location server to provide quality information for the provided SSR assistance data in the cases where a reference ephemeris is used other than the default ephemeris type used in *GNSS-SSR-URA*.

-- ASN1START

GNSS-SSR-URA-Set2-r17 ::= SEQUENCE {

refEph-r17 ENUMERATED { b1c,...},

gnss-SSR-URA-r17 GNSS-SSR-URA-r16,

...

}

-- ASN1STOP

| *GNSS-SSR-URA-Set2* field descriptions |
| --- |
| ***refEph***  This field specifies the reference ephemeris that quality information for the provided SSR assistance data refers to. In the case that *gnss-ID* indicates 'bds' and *refEph* indicates b1c, the SSR User Range Accuracy corrections are referenced to BDS B1C/B2a in table GNSS to iod Bit String (11) relation in IE GNSS‑NavigationModel (i.e. the B-CNAV1 broadcast ephemeris [52]). |
| ***gnss-SSR-URA***  This field specifies the quality information which refers to the reference ephemeris indicated by *refEph*. |

#### *– GNSS-LOS-NLOS-GriddedIndications*

The IE *GNSS-LOS-NLOS-GriddedIndications* is used by the location server to provide GNSS LOS-NLOS indication information. The parameters provided in IE *GNSS-LOS-NLOS-GriddedIndications* apply to all GNSSs.

-- ASN1START

GNSS-LOS-NLOS-GriddedIndications-r18 ::= SEQUENCE {

gridPointsSetID-r18 INTEGER (0..16383),

expirationTime-r18 UTCTime OPTIONAL, -- Need ON

gridList-r18 GridList-r18,

...

}

GridList-r18 ::= SEQUENCE (SIZE(1..1024)) OF GridElement-r18

GridElement-r18 ::= SEQUENCE {

gnss-LOS-InfoList-r18 GNSS-LOS-InfoList-r18 OPTIONAL, -- Need ON

...

}

GNSS-LOS-InfoList-r18 ::= SEQUENCE (SIZE(1..64)) OF GNSS-LOS-InfoElement-r18

GNSS-LOS-InfoElement-r18 ::= SEQUENCE {

svID-r18 SV-ID,

los-r18 ENUMERATED{true, false, uncertain},

...

}

-- ASN1STOP

| *GNSS-LOS-NLOS-GriddedIndications* field descriptions |
| --- |
| ***gridPointsSetID***  This field provides the ID of the LOS-NLOS Grid Point set. It is a regionally unique arbitrary number that is used by the UE to ensure that the GNSS LOS-NLOS indications are being applied to the correct set of points. |
| ***gridList***  This field provides the *GNSS LOS-NLOS* indications for up to 1024 grid points (up to 256 grid points per altitude layer) defined in the field *gnss-los-nlos-GridPoints* of IE *GNSS-CommonAssistData*.  The field *gnss-los-nlos-GridPoints* of IE *GNSS-CommonAssistData*, which is associated to this *gridPointsSetID*, includes the same number of entries as in the *gridList*, and listed in the same order, as defined by the enabled bits in the *bitmaskOfGrids*. The upmost grid layer is populated first, followed by the lower layer. |
| ***svID***  This field specifies the GNSS satellite for which the LOS-NLOS indications are provided. |
| ***los***  This field represents a LOS indication per svID per GNSS for a specific grid point, and can take the following values:  - true – the satellite vehicle is in line of sight  - false – the satellite vehicle is not in line of sight  - uncertain – satellite vehicle can either be in line of sight or not |
| ***expirationTime***  This field indicates when the validity of the provided assistance data fields expires. It is specified as UTC time. |

#### *– GNSS-SSR-SatellitePCVResiduals*

The IE *GNSS-SSR-SatellitePCVResiduals* is used by the location server to provide the nadir-angle-dependent phase center variations.

-- ASN1START

GNSS-SSR-SatellitePCVResiduals-r18 ::= SEQUENCE {

iod-ssr-PCVResiduals-r18 INTEGER (0..64),

ssr-SatellitePCV-List-r18 SSR-SatellitePCV-List-r18,

...

}

SSR-SatellitePCV-List-r18 ::= SEQUENCE (SIZE(1..64)) OF SSR-SatellitePCV-Element-r18

SSR-SatellitePCV-Element-r18 ::= SEQUENCE {

svID-r18 SV-ID,

ssr-SatellitePCV-FrequencyList-r18 SSR-SatellitePCV-FrequencyList-r18,

...

}

SSR-SatellitePCV-FrequencyList-r18 ::= SEQUENCE (SIZE(1..8)) OF

SSR-SatellitePCV-FrequencyElement-r18

SSR-SatellitePCV-FrequencyElement-r18 ::= SEQUENCE {

frequencyID-r18 GNSS-FrequencyID-r15,

phaseCenterVariations-r18 SSR-PhaseCenterVariationList-r18,

...

}

SSR-PhaseCenterVariationList-r18 ::= SEQUENCE (SIZE(1..32)) OF INTEGER(-1024..1023)

-- ASN1STOP

| *GNSS-SSR-SatellitePCVResiduals* field descriptions |
| --- |
| ***iod-ssr-PCVResiduals***  This field specifies the Issue of Data for the SSR Satellite PCV Residuals that is valid while the *GNSS-SSR-IOD-Update* is valid. |
| ***svID***  This field specifies the satellite for which the Satellite PCV Residual corrections are provided. |
| ***frequencyID***  This field specifies the satellite carrier frequency to which this correction applies. |
| ***phaseCenterVariations***  This field specifies the residual nadir only variations of the phase center that are not already accounted for within the SSR Phase Bias. The nadir angle is defined to be the angle away from the z-axis. The variations are given in increments of 1 degree steps, the first element is the variation at 1 degree.  In units of 1 mm. |

#### 6.5.2.3 GNSS Assistance Data Request

#### – *A-GNSS-RequestAssistanceData*

The IE *A-GNSS-RequestAssistanceData* is used by the target device to request GNSS assistance data from a location server.

-- ASN1START

A-GNSS-RequestAssistanceData ::= SEQUENCE {

gnss-CommonAssistDataReq GNSS-CommonAssistDataReq OPTIONAL, -- Cond CommonADReq

gnss-GenericAssistDataReq GNSS-GenericAssistDataReq OPTIONAL, -- Cond GenADReq

...,

[[

gnss-PeriodicAssistDataReq-r15

GNSS-PeriodicAssistDataReq-r15 OPTIONAL -- Cond PerADReq

]]

}

-- ASN1STOP

| Conditional presence | Explanation |
| --- | --- |
| *CommonADReq* | The field is mandatory present if the target device requests *GNSS-CommonAssistData*; otherwise it is not present. |
| *GenADReq* | This field is mandatory present if the target device requests *GNSS-GenericAssistData* for one or more specific GNSS; otherwise it is not present. |
| *PerADReq* | This field is mandatory present if the target device requests periodic GNSS assistance data delivery. This field may only be included if any of the fields are included in IE *GNSS‑GenericAssistDataReq:*  - *GNSS-RTK-ObservationsReq*,  - *GLO-RTK-BiasInformationReq*,  - *GNSS-RTK-MAC-CorrectionDifferencesReq*,  - *GNSS-RTK-ResidualsReq,*  - *GNSS-RTK-FKP-GradientsReq*,  - *GNSS-SSR-OrbitCorrectionsReq*,  - *GNSS-SSR-ClockCorrectionsReq*,  - *GNSS-SSR-CodeBiasReq.*  *- GNSS-SSR-URA-Req,*  *- GNSS-SSR-PhaseBiasReq,*  *- GNSS-SSR-STEC-CorrectionReq,*  *- GNSS-SSR-GriddedCorrectionReq,*  *- GNSS-Integrity-ServiceAlerReq,*  *- GNSS-SSR-OrbitCorrectionsSet2Req*,  *- GNSS-SSR-ClockCorrectionsSet2Req*,  *- GNSS-SSR-URA-Set2Req,* or  *- GNSS-SSR-IOD-UpdateReq.* |

#### – *GNSS-CommonAssistDataReq*

The IE *GNSS-CommonAssistDataReq* is used by the target device to request assistance data that are applicable to any GNSS from a location server.

-- ASN1START

GNSS-CommonAssistDataReq ::= SEQUENCE {

gnss-ReferenceTimeReq GNSS-ReferenceTimeReq

OPTIONAL, -- Cond RefTimeReq

gnss-ReferenceLocationReq GNSS-ReferenceLocationReq

OPTIONAL, -- Cond RefLocReq

gnss-IonosphericModelReq GNSS-IonosphericModelReq

OPTIONAL, -- Cond IonoModReq

gnss-EarthOrientationParametersReq GNSS-EarthOrientationParametersReq

OPTIONAL, -- Cond EOPReq

...,

[[

gnss-RTK-ReferenceStationInfoReq-r15

GNSS-RTK-ReferenceStationInfoReq-r15

OPTIONAL, -- Cond ARPReq

gnss-RTK-AuxiliaryStationDataReq-r15

GNSS-RTK-AuxiliaryStationDataReq-r15

OPTIONAL -- Cond AuxARPReq

]],

[[

gnss-SSR-CorrectionPointsReq-r16

GNSS-SSR-CorrectionPointsReq-r16

OPTIONAL -- Cond PointsReq

]],

[[

gnss-Integrity-ServiceParametersReq-r17

GNSS-Integrity-ServiceParametersReq-r17

OPTIONAL, -- Cond IntServiceReq

gnss-Integrity-ServiceAlertReq-r17

GNSS-Integrity-ServiceAlertReq-r17

OPTIONAL -- Cond IntAlertReq

]],

[[

gnss-SSR-IOD-UpdateReq-r18 GNSS-SSR-IOD-UpdateReq-r18

OPTIONAL -- Cond IODUpdateReq

]]

}

-- ASN1STOP

| Conditional presence | Explanation |
| --- | --- |
| *RefTimeReq* | The field is mandatory present if the target device requests *GNSS-ReferenceTime*; otherwise it is not present. |
| *RefLocReq* | This field is mandatory present if the target device requests *GNSS-ReferenceLocation*; otherwise it is not present. |
| *IonoModReq* | This field is mandatory present if the target device requests *GNSS-IonosphericModel*; otherwise it is not present. |
| *EOPReq* | This field is mandatory present if the target device requests *GNSS-EarthOrientationParameters*; otherwise it is not present. |
| *ARPReq* | This field is mandatory present if the target device requests *GNSS‑RTK‑ReferenceStationInfo*; otherwise it is not present. |
| *AuxARPReq* | This field is mandatory present if the target device requests *GNSS‑RTK‑AuxiliaryStationData*; otherwise it is not present. |
| *PointsReq* | This field is mandatory present if the target device requests *GNSS-SSR-CorrectionPoints*; otherwise it is not present. |
| *IntServiceReq* | This field is mandatory present if the target device requests *GNSS-Integrity-ServiceParameters*; otherwise it is not present. |
| *IntAlertReq* | This field is mandatory present if the target device requests *GNSS-Integrity-ServiceAlert*; otherwise it is not present. |
| *IODUpdateReq* | This field is mandatory present if the target device requests *GNSS-SSR-IOD-Update*; otherwise it is not present. |

#### – *GNSS-GenericAssistDataReq*

The IE *GNSS-GenericAssistDataReq* is used by the target device to request assistance data from a location server for one or more specific GNSSs. The specific GNSS for which the assistance data are requested is indicated by the IE *GNSS‑ID* and (if applicable) by the IE *SBAS‑ID*. Assistance for up to 16 GNSSs can be requested.

-- ASN1START

GNSS-GenericAssistDataReq ::= SEQUENCE (SIZE (1..16)) OF GNSS-GenericAssistDataReqElement

GNSS-GenericAssistDataReqElement ::= SEQUENCE {

gnss-ID GNSS-ID,

sbas-ID SBAS-ID OPTIONAL, -- Cond GNSS-ID-SBAS

gnss-TimeModelsReq GNSS-TimeModelListReq OPTIONAL, -- Cond TimeModReq

gnss-DifferentialCorrectionsReq GNSS-DifferentialCorrectionsReq OPTIONAL, -- Cond DGNSS-Req

gnss-NavigationModelReq GNSS-NavigationModelReq OPTIONAL, -- Cond NavModReq

gnss-RealTimeIntegrityReq GNSS-RealTimeIntegrityReq OPTIONAL, -- Cond RTIReq

gnss-DataBitAssistanceReq GNSS-DataBitAssistanceReq OPTIONAL, -- Cond DataBitsReq

gnss-AcquisitionAssistanceReq GNSS-AcquisitionAssistanceReq OPTIONAL, -- Cond AcquAssistReq

gnss-AlmanacReq GNSS-AlmanacReq OPTIONAL, -- Cond AlmanacReq

gnss-UTCModelReq GNSS-UTC-ModelReq OPTIONAL, -- Cond UTCModReq

gnss-AuxiliaryInformationReq GNSS-AuxiliaryInformationReq OPTIONAL, -- Cond AuxInfoReq

...,

[[

bds-DifferentialCorrectionsReq-r12

BDS-DifferentialCorrectionsReq-r12

OPTIONAL, -- Cond DBDS-Req

bds-GridModelReq-r12 BDS-GridModelReq-r12 OPTIONAL -- Cond BDS-GridModReq

]],

[[

gnss-RTK-ObservationsReq-r15

GNSS-RTK-ObservationsReq-r15 OPTIONAL, -- Cond RTK-OSR-Req

glo-RTK-BiasInformationReq-r15

GLO-RTK-BiasInformationReq-r15 OPTIONAL, -- Cond GLO-CPB-Req

gnss-RTK-MAC-CorrectionDifferencesReq-r15

GNSS-RTK-MAC-CorrectionDifferencesReq-r15

OPTIONAL, -- Cond MAC-Req

gnss-RTK-ResidualsReq-r15 GNSS-RTK-ResidualsReq-r15 OPTIONAL, -- Cond Res-Req

gnss-RTK-FKP-GradientsReq-r15

GNSS-RTK-FKP-GradientsReq-r15 OPTIONAL, -- Cond FKP-Req

gnss-SSR-OrbitCorrectionsReq-r15

GNSS-SSR-OrbitCorrectionsReq-r15

OPTIONAL, -- Cond OC-Req

gnss-SSR-ClockCorrectionsReq-r15

GNSS-SSR-ClockCorrectionsReq-r15

OPTIONAL, -- Cond CC-Req

gnss-SSR-CodeBiasReq-r15 GNSS-SSR-CodeBiasReq-r15 OPTIONAL -- Cond CB-Req

]],

[[

gnss-SSR-URA-Req-r16 GNSS-SSR-URA-Req-r16 OPTIONAL, -- Cond URA-Req

gnss-SSR-PhaseBiasReq-r16 GNSS-SSR-PhaseBiasReq-r16 OPTIONAL, -- Cond PB-Req

gnss-SSR-STEC-CorrectionReq-r16

GNSS-SSR-STEC-CorrectionReq-r16 OPTIONAL, -- Cond STEC-Req

gnss-SSR-GriddedCorrectionReq-r16 GNSS-SSR-GriddedCorrectionReq-r16

OPTIONAL, -- Cond Grid-Req

navic-DifferentialCorrectionsReq-r16

NavIC-DifferentialCorrectionsReq-r16

OPTIONAL, -- Cond DNavIC-Req

navic-GridModelReq-r16 NavIC-GridModelReq-r16 OPTIONAL -- Cond NavIC-GridModReq

]],

[[

gnss-SSR-OrbitCorrectionsSet2Req-r17

GNSS-SSR-OrbitCorrectionsSet2Req-r17

OPTIONAL, -- Cond OC2-Req

gnss-SSR-ClockCorrectionsSet2Req-r17

GNSS-SSR-ClockCorrectionsSet2Req-r17

OPTIONAL, -- Cond CC2-Req

gnss-SSR-URA-Set2Req-r17 GNSS-SSR-URA-Set2Req-r17 OPTIONAL -- Cond URA2-Req

]],

[[

gnss-LOS-NLOS-GriddedIndicationsReq-r18 GNSS-LOS-NLOS-GriddedIndicationsReq-r18

OPTIONAL, -- Cond LOS-GridReq

gnss-SSR-SatellitePCVResidualsReq-r18

GNSS-SSR-SatellitePCVResidualsReq-r18

OPTIONAL -- Cond SatPCV-Req

]]

}

-- ASN1STOP

| Conditional presence | Explanation |
| --- | --- |
| *GNSS‑ID‑SBAS* | The field is mandatory present if the *GNSS‑ID* = *sbas*; otherwise it is not present. |
| *TimeModReq* | The field is mandatory present if the target device requests *GNSS-TimeModelList*; otherwise it is not present. |
| *DGNSS-Req* | The field is mandatory present if the target device requests *GNSS-DifferentialCorrections*; otherwise it is not present. |
| *NavModReq* | The field is mandatory present if the target device requests *GNSS-NavigationModel*; otherwise it is not present. |
| *RTIReq* | The field is mandatory present if the target device requests *GNSS-RealTimeIntegrity*; otherwise it is not present. |
| *DataBitsReq* | The field is mandatory present if the target device requests *GNSS-DataBitAssistance*; otherwise it is not present. |
| *AcquAssistReq* | The field is mandatory present if the target device requests *GNSS-AcquisitionAssistance*; otherwise it is not present. |
| *AlmanacReq* | The field is mandatory present if the target device requests *GNSS-Almanac*; otherwise it is not present. |
| *UTCModReq* | The field is mandatory present if the target device requests *GNSS-UTCModel*; otherwise it is not present. |
| *AuxInfoReq* | The field is mandatory present if the target device requests *GNSS-AuxiliaryInformation*; otherwise it is not present. |
| *DBDS-Req* | The field is mandatory present if the target device requests *BDS-DifferentialCorrections*; otherwise it is not present. This field may only be present if *gnss-ID* indicates 'bds'. |
| *BDS-GridModReq* | The field is mandatory present if the target device requests *BDS-GridModel*; otherwise it is not present. This field may only be present if *gnss-ID* indicates 'bds'. |
| *RTK-OSR-Req* | The field is mandatory present if the target device requests *GNSS-RTK-Observations*; otherwise it is not present. |
| *GLO-CPB-Req* | The field is mandatory present if the target device requests *GLO-RTK-BiasInformation*; otherwise it is not present. |
| *MAC-Req* | The field is mandatory present if the target device requests *GNSS‑RTK‑MAC‑CorrectionDifferences*; otherwise it is not present. |
| *Res-Req* | The field is mandatory present if the target device requests *GNSS-RTK-Residuals*; otherwise it is not present. |
| *FKP-Req* | The field is mandatory present if the target device requests *GNSS-RTK-FKP-Gradients*; otherwise it is not present. |
| *OC-Req* | The field is mandatory present if the target device requests *GNSS-SSR-OrbitCorrections*; otherwise it is not present. |
| *CC-Req* | The field is mandatory present if the target device requests *GNSS-SSR-ClockCorrections*; otherwise it is not present. |
| *CB-Req* | The field is mandatory present if the target device requests *GNSS-SSR-CodeBias*; otherwise it is not present. |
| *URA-Req* | The field is mandatory present if the target device requests *GNSS-SSR-URA*; otherwise it is not present. |
| *PB-Req* | The field is mandatory present if the target device requests *GNSS-SSR-PhaseBias*; otherwise it is not present. |
| *STEC-Req* | The field is mandatory present if the target device requests *GNSS-SSR-STEC-Correction*; otherwise it is not present. |
| *Grid-Req* | The field is mandatory present if the target device requests *GNSS‑SSR‑GriddedCorrection*; otherwise it is not present. |
| *DNavIC-Req* | The field is mandatory present if the target device requests *NavIC-DifferentialCorrections*; otherwise it is not present. This field may only be present if the *gnss-ID* indicates 'navic'. |
| *NavIC-GridModReq* | The field is mandatory present if the target device requests *NavIC-GridModel*; otherwise it is not present. This field may only be present if the *gnss-ID* indicates 'navic'. |
| *OC2-Req* | The field is mandatory present if the target device requests *GNSS-SSR-OrbitCorrectionsSet2*; otherwise it is not present. |
| *CC2-Req* | The field is mandatory present if the target device requests *GNSS-SSR-ClockCorrectionsSet2*; otherwise it is not present. |
| *URA2-Req* | The field is mandatory present if the target device requests *GNSS-SSR-URA-Set2*; otherwise it is not present. |
| *LOS-GridReq* | The field is mandatory present if the target device requests *GNSS-LOS-NLOS-GriddedIndications*; otherwise it is not present. |
| *SatPCV-Req* | The field is mandatory present if the target device requests *GNSS-SSR-SatellitePCVResiduals*; otherwise it is not present. |

#### *– GNSS-PeriodicAssistDataReq*

The IE *GNSS-PeriodicAssistDataReq* is used by the target device to request periodic assistance data delivery from a location server.

-- ASN1START

GNSS-PeriodicAssistDataReq-r15 ::= SEQUENCE {

gnss-RTK-PeriodicObservationsReq-r15 GNSS-PeriodicControlParam-r15 OPTIONAL, -- Cond pOSR

glo-RTK-PeriodicBiasInformationReq-r15 GNSS-PeriodicControlParam-r15 OPTIONAL, -- Cond pCPB

gnss-RTK-MAC-PeriodicCorrectionDifferencesReq-r15

GNSS-PeriodicControlParam-r15 OPTIONAL, -- Cond pMAC

gnss-RTK-PeriodicResidualsReq-r15 GNSS-PeriodicControlParam-r15 OPTIONAL, -- Cond pRes

gnss-RTK-FKP-PeriodicGradientsReq-r15 GNSS-PeriodicControlParam-r15 OPTIONAL, -- Cond pFKP

gnss-SSR-PeriodicOrbitCorrectionsReq-r15

GNSS-PeriodicControlParam-r15 OPTIONAL, -- Cond pOC

gnss-SSR-PeriodicClockCorrectionsReq-r15

GNSS-PeriodicControlParam-r15 OPTIONAL, -- Cond pCC

gnss-SSR-PeriodicCodeBiasReq-r15 GNSS-PeriodicControlParam-r15 OPTIONAL, -- Cond pCB

...,

[[

gnss-SSR-PeriodicURA-Req-r16 GNSS-PeriodicControlParam-r15 OPTIONAL, -- Cond pURA

gnss-SSR-PeriodicPhaseBiasReq-r16 GNSS-PeriodicControlParam-r15 OPTIONAL, -- Cond pPB

gnss-SSR-PeriodicSTEC-CorrectionReq-r16 GNSS-PeriodicControlParam-r15 OPTIONAL, -- Cond pSTEC

gnss-SSR-PeriodicGriddedCorrectionReq-r16

GNSS-PeriodicControlParam-r15 OPTIONAL -- Cond pGrid

]],

[[

gnss-Integrity-PeriodicServiceAlertReq-r17

GNSS-PeriodicControlParam-r15 OPTIONAL -- Cond pDNU

]],

[[

gnss-SSR-PeriodicOrbitCorrectionsSet2Req-r17

GNSS-PeriodicControlParam-r15 OPTIONAL, -- Cond pOC2

gnss-SSR-PeriodicClockCorrectionsSet2Req-r17

GNSS-PeriodicControlParam-r15 OPTIONAL, -- Cond pCC2

gnss-SSR-PeriodicURA-Set2Req-r17

GNSS-PeriodicControlParam-r15 OPTIONAL -- Cond pURA2

]],

[[

gnss-SSR-PeriodicIOD-UpdateReq-r18

GNSS-PeriodicControlParam-r15 OPTIONAL -- Cond pPCV

]]

}

-- ASN1STOP

| *Conditional presence* | Explanation |
| --- | --- |
| *pOSR* | The field is mandatory present if the target device requests periodic *GNSS‑RTK‑Observations*; otherwise it is not present. |
| *pCPB* | The field is mandatory present if the target device requests periodic *GLO‑RTK‑BiasInformation*; otherwise it is not present. |
| *pMAC* | The field is mandatory present if the target device requests periodic *GNSS‑RTK‑MAC‑CorrectionDifferences*; otherwise it is not present. |
| *pRes* | The field is mandatory present if the target device requests periodic *GNSS‑RTK‑Residuals*; otherwise it is not present. |
| *pFKP* | The field is mandatory present if the target device requests periodic *GNSS‑RTK‑FKP‑Gradients*; otherwise it is not present. |
| *pOC* | The field is mandatory present if the target device requests periodic *GNSS‑SSR‑OrbitCorrections*; otherwise it is not present. |
| *pCC* | The field is mandatory present if the target device requests periodic *GNSS‑SSR‑ClockCorrections*; otherwise it is not present. |
| *pCB* | The field is mandatory present if the target device requests periodic *GNSS‑SSR‑CodeBias*; otherwise it is not present. |
| *pURA* | The field is mandatory present if the target device requests periodic *GNSS‑SSR‑URA*; otherwise it is not present. |
| *pPB* | The field is mandatory present if the target device requests periodic *GNSS‑SSR‑PhaseBias*; otherwise it is not present. |
| *pSTEC* | The field is mandatory present if the target device requests periodic *GNSS‑SSR‑STEC‑Correction*; otherwise it is not present. |
| *pGrid* | The field is mandatory present if the target device requests periodic *GNSS‑SSR‑GriddedCorrection*; otherwise it is not present. |
| *pDNU* | The field is mandatory present if the target device requests periodic *GNSS-Integrity-ServiceAlert*; otherwise it is not present. |
| *pOC2* | The field is mandatory present if the target device requests periodic *GNSS‑SSR‑OrbitCorrectionsSet2*; otherwise it is not present. |
| *pCC2* | The field is mandatory present if the target device requests periodic *GNSS‑SSR‑ClockCorrectionsSet2*; otherwise it is not present. |
| *pURA2* | The field is mandatory present if the target device requests periodic *GNSS‑SSR‑URA-Set2*; otherwise it is not present. |
| *pPCV* | The field is mandatory present if the target device requests periodic *GNSS SSR IOD-Update*; otherwise it is not present. |

#### 6.5.2.4 GNSS Assistance Data Request Elements

#### – *GNSS-ReferenceTimeReq*

The IE *GNSS-ReferenceTimeReq* is used by the target device to request the *GNSS-ReferenceTime* assistance from the location server.

-- ASN1START

GNSS-ReferenceTimeReq ::= SEQUENCE {

gnss-TimeReqPrefList SEQUENCE (SIZE (1..8)) OF GNSS-ID,

gps-TOW-assistReq BOOLEAN OPTIONAL, -- Cond gps

notOfLeapSecReq BOOLEAN OPTIONAL, -- Cond glonass

...

}

-- ASN1STOP

| Conditional presence | Explanation |
| --- | --- |
| *gps* | The field is mandatory present if *gnss-TimeReqPrefList* includes a *GNSS-ID*= 'gps'; otherwise it is not present. |
| *glonass* | The field is mandatory present if *gnss-TimeReqPrefList* includes a *GNSS-ID*= 'glonass'; otherwise it is not present. |

| *GNSS-ReferenceTimeReq* field descriptions |
| --- |
| ***gnss-TimeReqPrefList***  This field is used by the target device to request the system time for a specific GNSS, specified by GNSS-ID in the order of preference. The first *GNSS-ID* in the list is the most preferred GNSS for reference time, the second *GNSS-ID* is the second most preferred, etc. |
| ***gps-TOW-assistReq***  This field is used by the target device to request the *gps-TOW-Assist* field in *GNSS-SystemTime*. TRUE means requested. |
| ***notOfLeapSecReq***  This field is used by the target device to request the *notificationOfLeapSecond* field in *GNSS-SystemTime*. TRUE means requested. |

#### – *GNSS-ReferenceLocationReq*

The IE *GNSS-ReferenceLocationReq* is used by the target device to request the *GNSS-ReferenceLocation* assistancefrom the location server.

-- ASN1START

GNSS-ReferenceLocationReq ::= SEQUENCE {

...

}

-- ASN1STOP

#### – *GNSS-IonosphericModelReq*

The IE *GNSS-IonosphericModelReq* is used by the target device to request the *GNSS-IonosphericModel* assistancefrom the location server.

-- ASN1START

GNSS-IonosphericModelReq ::= SEQUENCE {

klobucharModelReq BIT STRING (SIZE(2)) OPTIONAL, -- Cond klobuchar

neQuickModelReq NULL OPTIONAL, -- Cond nequick

...,

[[ klobucharModel2Req-r16 NULL OPTIONAL -- Cond klobuchar2

]]

}

-- ASN1STOP

| Conditional presence | Explanation |
| --- | --- |
| *klobuchar* | The field is mandatory present if the target device requests *klobucharModel*; otherwise it is not present. The BIT STRING defines the *dataID* requested, defined in IE *KlobucharModelParameter*. |
| *nequick* | The field is mandatory present if the target device requests *neQuickModel*; otherwise it is not present. |
| *klobuchar2* | The field is mandatory present if the target device requests *klobucharModel2*; otherwise it is not present. |

#### – *GNSS-EarthOrientationParametersReq*

The IE *GNSS-EarthOrientationParametersReq* is used by the target device to request the *GNSS-EarthOrientationParameters* assistancefrom the location server.

-- ASN1START

GNSS-EarthOrientationParametersReq ::= SEQUENCE {

...

}

-- ASN1STOP

#### *– GNSS-RTK-ReferenceStationInfoReq*

The IE *GNSS-RTK-ReferenceStationInfoReq* is used by the target device to request the *GNSS‑RTK‑ReferenceStationInfo* assistancefrom the location server.

-- ASN1START

GNSS-RTK-ReferenceStationInfoReq-r15 ::= SEQUENCE {

antennaDescriptionReq-r15 BOOLEAN,

antennaHeightReq-r15 BOOLEAN,

physicalReferenceStationReq-r15 BOOLEAN,

stationID-r15 GNSS-ReferenceStationID-r15 OPTIONAL,

...

}

-- ASN1STOP

| *GNSS-RTK-ReferenceStationInfoReq* field descriptions |
| --- |
| ***antennaDescriptionReq***  This field specifies whether or not the location server is requested to include the field *AntennaDescription* in the *GNSS-RTK-ReferenceStationInfo* IE. TRUE means requested. |
| ***antennaHeightReq***  This field specifies whether or not the location server is requested to include the field *antennaHeight* in the *GNSS‑RTK-ReferenceStationInfo* IE. TRUE means requested. |
| ***physicalReferenceStationReq***  This field specifies whether or not the location server is requested to include the field *physical-reference-station-info* in the *GNSS‑RTK-ReferenceStationInfo* IE. TRUE means requested. |
| ***stationID***  This field specifies the Station ID for which the *GNSS-RTK-ReferenceStationInfo* is requested. |

#### *– GNSS-RTK-AuxiliaryStationDataReq*

The IE *GNSS-RTK-AuxiliaryStationDataReq* is used by the target device to request the *GNSS‑RTK‑AuxiliaryStationData* assistancefrom the location server.

-- ASN1START

GNSS-RTK-AuxiliaryStationDataReq-r15 ::= SEQUENCE {

master-referenceStationID-r15 GNSS-ReferenceStationID-r15 OPTIONAL,

...

}

-- ASN1STOP

| *GNSS-RTK-AuxiliaryStationDataReq* field descriptions |
| --- |
| ***master-referenceStationID***  This field specifies the Master Reference Station ID for which the Auxiliary Stations are requested. |

#### – *GNSS-SSR-CorrectionPointsReq*

The IE *GNSS-SSR-CorrectionPointsReq* is used by the target device to request the *GNSS-SSR-CorrectionPoints* assistancefrom the location server.

-- ASN1START

GNSS-SSR-CorrectionPointsReq-r16 ::= SEQUENCE {

correctionPointSetID-Req-r16 INTEGER (0..16383) OPTIONAL,

...

}

-- ASN1STOP

| *GNSS-SSR-CorrectionPointsReq* field descriptions |
| --- |
| ***correctionPointSetID-Req***  This field specifies the ID of the Atmospheric Correction Point set for which the *GNSS-SSR-CorrectionPoints* are requested. |

#### – *GNSS-Integrity-ServiceParametersReq*

The IE *GNSS-Integrity-ServiceParametersReq* is used by the target device to request the *GNSS-Integrity-ServiceParameters* assistancefrom the location server.

-- ASN1START

GNSS-Integrity-ServiceParametersReq-r17 ::= SEQUENCE {

...

}

-- ASN1STOP

#### – *GNSS-Integrity-ServiceAlertReq*

The IE *GNSS-Integrity-ServiceAlertReq* is used by the target device to request the *GNSS-Integrity-ServiceAlert* assistancefrom the location server.

-- ASN1START

GNSS-Integrity-ServiceAlertReq-r17 ::= SEQUENCE {

...

}

-- ASN1STOP

#### – *GNSS-SSR-IOD-UpdateReq*

The IE *GNSS-SSR-IOD-UpdateReq* is used by the target device to request the *GNSS-SSR-IOD-Update* assistancefrom the location server.

-- ASN1START

GNSS-SSR-IOD-UpdateReq-r18 ::= SEQUENCE {

...

}

-- ASN1STOP

#### – *GNSS-TimeModelListReq*

The IE *GNSS-TimeModelListReq* is used by the target device to request the *GNSS-TimeModelElement* assistancefrom the location server.

-- ASN1START

GNSS-TimeModelListReq ::= SEQUENCE (SIZE(1..15)) OF GNSS-TimeModelElementReq

GNSS-TimeModelElementReq ::= SEQUENCE {

gnss-TO-IDsReq INTEGER (1..15),

deltaTreq BOOLEAN,

...

}

-- ASN1STOP

| *GNSS-TimeModelElementReq* field descriptions |
| --- |
| ***gnss-TO-IDsReq***  This field specifies the requested *gnss-TO-ID*. The meaning and encoding is the same as the *gnss-TO-ID* field in the *GNSS-TimeModelElement* IE. |
| ***deltaTreq***  This field specifies whether or not the location server is requested to include the *deltaT* field in the *GNSS-TimeModelElement* IE. TRUE means requested. |

#### – *GNSS-DifferentialCorrectionsReq*

The IE *GNSS-DifferentialCorrectionsReq* is used by the target device to request the *GNSS-DifferentialCorrections* assistancefrom the location server.

-- ASN1START

GNSS-DifferentialCorrectionsReq ::= SEQUENCE {

dgnss-SignalsReq GNSS-SignalIDs,

dgnss-ValidityTimeReq BOOLEAN,

...

}

-- ASN1STOP

| *GNSS-DifferentialCorrectionsReq* field descriptions |
| --- |
| ***dgnss-SignalsReq***  This field specifies the GNSS Signal(s) for which the *GNSS-DifferentialCorrections* are requested. A one‑value at a bit position means DGNSS corrections for the specific signal are requested; a zero‑value means not requested. The target device shall set a maximum of three bits to value 'one'. |
| ***dgnss-ValidityTimeReq***  This field specifies whether the *udreGrowthRate* and *udreValidityTime* in *GNSS-DifferentialCorrections* are requested or not. TRUE means requested. |

#### – *GNSS-NavigationModelReq*

The IE *GNSS-NavigationModelReq* is used by the target device to request the *GNSS-NavigationModel* assistancefrom the location server.

-- ASN1START

GNSS-NavigationModelReq ::= CHOICE {

storedNavList StoredNavListInfo,

reqNavList ReqNavListInfo,

...

}

StoredNavListInfo ::= SEQUENCE {

gnss-WeekOrDay INTEGER (0..4095),

gnss-Toe INTEGER (0..255),

t-toeLimit INTEGER (0..15),

satListRelatedDataList SatListRelatedDataList OPTIONAL,

...

}

SatListRelatedDataList ::= SEQUENCE (SIZE (1..64)) OF SatListRelatedDataElement

SatListRelatedDataElement ::= SEQUENCE {

svID SV-ID,

iod BIT STRING (SIZE(11)),

clockModelID INTEGER (1..8) OPTIONAL,

orbitModelID INTEGER (1..8) OPTIONAL,

...

}

ReqNavListInfo ::= SEQUENCE {

svReqList BIT STRING (SIZE (64)),

clockModelID-PrefList SEQUENCE (SIZE (1..8)) OF INTEGER (1..8) OPTIONAL,

orbitModelID-PrefList SEQUENCE (SIZE (1..8)) OF INTEGER (1..8) OPTIONAL,

addNavparamReq BOOLEAN OPTIONAL, -- Cond orbitModelID-2

...

}

-- ASN1STOP

| Conditional presence | Explanation |
| --- | --- |
| *orbitModelID-2* | The field is mandatory present if *orbitModelID-PrefList* is absent or includes a Model-ID = '2'; otherwise it is not present. |

| *GNSS-NavigationModelReq* field descriptions |
| --- |
| ***storedNavList***  This list provides information to the location server about which *GNSS-NavigationModel* data the target device has currently stored for the particular GNSS indicated by *GNSS-ID*. |
| ***reqNavList***  This list provides information to the location server which *GNSS-NavigationModel* data are requested by the target device. |
| ***gnss-WeekOrDay***  If *GNSS-ID* does not indicate 'glonass', this field defines the GNSS Week number of the assistance currently held by the target device.  If *GNSS-ID* is set to 'glonass', this field defines the calendar number of day within the four-year interval starting from 1st of January in a leap year, as defined by the parameter NT in [9] of the assistance currently held by the target device. |
| ***gnss-Toe***  If *GNSS-ID* does not indicate 'glonass', this field defines the GNSS time of ephemeris in hours of the latest ephemeris set contained by the target device.  If *GNSS-ID* is set to 'glonass', this field defines the time of ephemeris in units of 15 minutes of the latest ephemeris set contained by the target device (range 0 to 95 representing time values between 0 and 1425 minutes). In this case, values 96 to 255 shall not be used by the sender. |
| ***t-toeLimit***  If *GNSS-ID* does not indicate 'glonass', this IE defines the ephemeris age tolerance of the target device in units of hours.  If *GNSS-ID* is set to 'glonass', this IE defines the ephemeris age tolerance of the target device in units of 30 minutes. |
| ***satListRelatedDataList***  This list defines the clock and orbit models currently held by the target device for each SV. This field is not included if the target device does not have any stored clock and orbit models for any SV. |
| ***svID***  This field identifies the particular GNSS satellite. |
| ***iod***  This field identifies the issue of data currently held by the target device. |
| ***clockModelID, orbitModelID***  These fields define the clock and orbit model number currently held by the target device. If these fields are absent, the default interpretation of the table GNSS-ID to clockModelID & orbitModelID relation below applies. |
| ***svReqList***  This field defines the SV for which the navigation model assistance is requested. Each bit position in this BIT STRING represents a *SV-ID*. Bit 0 represents *SV-ID*=0 and bit 63 represents *SV-ID*=63. A one-value at a bit position means the navigation model data for the corresponding *SV-ID* is requested, a zero-value means not requested. |
| ***clockModelIDPrefList, orbitModelID-PrefList***  These fields define the Model-IDs of the clock and orbit models that the target device wishes to obtain in the order of preference. The first Model-ID in the list is the most preferred model, the second Model-ID the second most preferred, etc. If these fields are absent, the default interpretation of the table GNSS-ID to clockModelID-PrefList & orbitModelIDPrefList relation below applies. |
| ***addNavparamReq***  This field specifies whether the location server is requested to include the *addNAVparam* fields in *GNSS-NavigationModel* IE (*NavModel-NAVKeplerianSet* field) or not. TRUE means requested. |

GNSS-ID to clockModelID & orbitModelID relation

|  |  |  |
| --- | --- | --- |
| *GNSS-ID* | *clockModelID* | *orbitModelID* |
| gps | 2 | 2 |
| sbas | 5 | 5 |
| qzss | 2 | 2 |
| galileo | 1 | 1 |
| glonass | 4 | 4 |
| bds | 6 | 6 |
| navic | 8 | 8 |

GNSS-ID to clockModelID-PrefList & orbitModelID-PrefList relation

|  |  |  |
| --- | --- | --- |
| *GNSS-ID* | *clockModelID-PrefList* | *orbitModelID-PrefList* |
| gps | Model-2 | Model-2 |
| sbas | Model-5 | Model-5 |
| qzss | Model-2 | Model-2 |
| galileo | Model-1 | Model-1 |
| glonass | Model-4 | Model-4 |
| bds | Model-6 | Model-6 |
| navic | Model-8 | Model-8 |

#### – *GNSS-RealTimeIntegrityReq*

The IE *GNSS-RealTimeIntegrityReq* is used by the target device to request the *GNSS-RealTimeIntegrity* assistancefrom the location server.

-- ASN1START

GNSS-RealTimeIntegrityReq ::= SEQUENCE {

...

}

-- ASN1STOP

#### – *GNSS-DataBitAssistanceReq*

The IE *GNSS-DataBitAssistanceReq* is used by the target device to request the *GNSS-DataBitAssistance* assistancefrom the location server.

-- ASN1START

GNSS-DataBitAssistanceReq ::= SEQUENCE {

gnss-TOD-Req INTEGER (0..3599),

gnss-TOD-FracReq INTEGER (0..999) OPTIONAL,

dataBitInterval INTEGER (0..15),

gnss-SignalType GNSS-SignalIDs,

gnss-DataBitsReq GNSS-DataBitsReqSatList OPTIONAL,

...

}

GNSS-DataBitsReqSatList ::= SEQUENCE (SIZE(1..64)) OF GNSS-DataBitsReqSatElement

GNSS-DataBitsReqSatElement ::= SEQUENCE {

svID SV-ID,

...

}

-- ASN1STOP

| *GNSS-DataBitAssistanceReq* field descriptions |
| --- |
| ***gnss-TOD-Req***  This field specifies the reference time for the first data bit requested in GNSS specific system time, modulo 1 hour.  Scale factor 1 second. |
| ***gnss-TOD-FracReq***  This field specifies the fractional part of *gnss-TOD-Req* in 1-milli‑second resolution.  Scale factor 1 millisecond. |
| ***dataBitInterval***  This field specifies the time length for which the Data Bit Assistance is requested. The *GNSS-DataBitAssistance* shall be relative to the time interval (*gnss-TOD-Req*, *gnss-TOD-Req* + *dataBitInterval*).  The *dataBitInterval**r*, expressed in seconds, is mapped to a binary number K with the following formula:  *r* =0.1 × 2 K  Value K=15 means that the time interval is not specified. |
| ***gnss-SignalType***  This field specifies the GNSS Signal(s) for which the *GNSS-DataBitAssistance* are requested. A one‑value at a bit position means *GNSS-DataBitAssistance* for the specific signal is requested; a zero‑value means not requested. |
| ***gnss-DataBitsReq***  This list contains the SV-IDs for which the *GNSS-DataBitAssistance* is requested. |

#### – *GNSS-AcquisitionAssistanceReq*

The IE *GNSS-AcquisitionAssistanceReq* is used by the target device to request the *GNSS-AcquisitionAssistance* assistancefrom the location server.

-- ASN1START

GNSS-AcquisitionAssistanceReq ::= SEQUENCE {

gnss-SignalID-Req GNSS-SignalID,

...

}

-- ASN1STOP

| *GNSS-AcquisitionAssistanceReq* field descriptions |
| --- |
| ***gnss-SignalID-Req***  This field specifies the GNSS signal type for which *GNSSAcquisitionAssistance* is requested. |

#### – *GNSS-AlmanacReq*

The IE *GNSS-AlmanacReq* is used by the target device to request the *GNSS-Almanac* assistancefrom the location server.

-- ASN1START

GNSS-AlmanacReq ::= SEQUENCE {

modelID INTEGER(1..8) OPTIONAL,

...

}

-- ASN1STOP

| *GNSS-AlmanacReq* field descriptions |
| --- |
| ***modelID***  This field specifies the Almanac Model ID requested. If this field is absent, the default interpretation as in the table GNSS-ID to modelID relation below applies. |

GNSS-ID to modelID relation

|  |  |
| --- | --- |
| *GNSS-ID* | *modelID* |
| gps | 2 |
| sbas | 6 |
| qzss | 2 |
| galileo | 1 |
| glonass | 5 |
| bds | 7 |
| navic | 8 |

#### – *GNSS-UTC-ModelReq*

The IE *GNSS-UTC-ModelReq* is used by the target device to request the *GNSS-UTC-Model* assistancefrom the location server.

-- ASN1START

GNSS-UTC-ModelReq ::= SEQUENCE {

modelID INTEGER(1..8) OPTIONAL,

...

}

-- ASN1STOP

| *GNSS-UTC-ModelReq* field descriptions |
| --- |
| ***modelID***  This field specifies the *GNSS-UTCModel* set requested. If this field is absent, the default interpretation as in the table GNSS-ID to modelID relation below applies. |

GNSS-ID to modelID relation

|  |  |
| --- | --- |
| *GNSS-ID* | *modelID* |
| gps | 1 |
| sbas | 4 |
| qzss | 1 |
| galileo | 1 |
| glonass | 3 |
| bds | 5 |
| navic | 2 |

#### – *GNSS-AuxiliaryInformationReq*

The IE *GNSS-AuxiliaryInformationReq* is used by the target device to request the *GNSS-AuxiliaryInformation* assistancefrom the location server.

-- ASN1START

GNSS-AuxiliaryInformationReq ::= SEQUENCE {

...

}

-- ASN1STOP

#### – *BDS-DifferentialCorrectionsReq*

The IE *BDS-DifferentialCorrectionsReq* is used by the target device to request the *BDS-DifferentialCorrections* assistancefrom the location server.

-- ASN1START

BDS-DifferentialCorrectionsReq-r12 ::= SEQUENCE {

dgnss-SignalsReq GNSS-SignalIDs,

...

}

-- ASN1STOP

| *BDS-DifferentialCorrectionsReq* field descriptions |
| --- |
| ***dgnss-SignalsReq***  This field specifies the BDS Signal(s) for which the *BDS-DifferentialCorrections* are requested. A one‑value at a bit position means BDS differential corrections for the specific signal are requested; a zero‑value means not requested. The target device shall set a maximum of three bits to value 'one'. This only applies for the B1I/B3I signal. |

#### – *BDS-GridModelReq*

The IE *BDS-GridModelReq* is used by the target device to request the *BDS-GridModel* assistancefrom the location server.

-- ASN1START

BDS-GridModelReq-r12 ::= SEQUENCE {

...

}

-- ASN1STOP

#### *– GNSS-RTK-ObservationsReq*

The IE *GNSS-RTK-ObservationsReq* is used by the target device to request the *GNSS-RTK-Observations* assistancefrom the location server.

-- ASN1START

GNSS-RTK-ObservationsReq-r15::= SEQUENCE {

gnss-RTK-SignalsReq-r15 GNSS-SignalIDs,

gnss-RTK-Integer-ms-Req-r15 BOOLEAN,

gnss-RTK-PhaseRangeRateReq-r15 BOOLEAN,

gnss-RTK-CNR-Req-r15 BOOLEAN,

stationID-r15 GNSS-ReferenceStationID-r15 OPTIONAL,

...

}

-- ASN1STOP

| *GNSS-RTK-ObservationsReq* field descriptions |
| --- |
| ***gnss-RTK-SignalsReq***  This field specifies the GNSS Signal(s) for which the *GNSS-RTK-Observations* are requested. A one‑value at a bit position means RTK observations for the specific signal are requested; a zero‑value means not requested. |
| ***gnss-RTK-Integer-ms-Req***  This field specifies whether the integer-ms is requested or not. TRUE means requested. |
| ***gnss-RTK-PhaseRangeRateReq***  This field specifies whether the *rough-phase-range-rate* and *fine-PhaseRangeRate* are requested or not. TRUE means requested. |
| ***gnss-RTK-CNR-Req***  This field specifies whether the *carrier-to-noise-ratio* is requested or not. TRUE means requested. |
| ***stationID***  This field specifies the Station ID for which the GNSS-RTK-Observations are requested. |

#### *– GLO-RTK-BiasInformationReq*

The IE *GLO-RTK-BiasInformationReq* is used by the target device to request the *GLO-RTK-BiasInformation* assistancefrom the location server.

-- ASN1START

GLO-RTK-BiasInformationReq-r15 ::= SEQUENCE {

stationID-r15 GNSS-ReferenceStationID-r15 OPTIONAL,

...

}

-- ASN1STOP

| *GLO-RTK-BiasInformationReq* field descriptions |
| --- |
| ***stationID***  This field specifies the Station ID for which the *GLO-RTK-BiasInformation* is requested. |

#### *– GNSS-RTK-MAC-CorrectionDifferencesReq*

The IE *GNSS-RTK-MAC-CorrectionDifferencesReq* is used by the target device to request the *GNSS‑RTK‑MAC‑CorrectionDifferences* assistancefrom the location server.

-- ASN1START

GNSS-RTK-MAC-CorrectionDifferencesReq-r15 ::= SEQUENCE {

master-ReferenceStationID-r15 GNSS-ReferenceStationID-r15 OPTIONAL,

aux-ReferenceStationList-r15 AUX-ReferenceStationList-r15 OPTIONAL,

linkCombinations-PrefList-r15 GNSS-Link-CombinationsList-r15 OPTIONAL,

...

}

AUX-ReferenceStationList-r15 ::= SEQUENCE (SIZE (1..32)) OF AUX-ReferenceStationID-Element-r15

AUX-ReferenceStationID-Element-r15 ::= SEQUENCE {

aux-stationID-r15 GNSS-ReferenceStationID-r15,

...

}

-- ASN1STOP

| *GNSS-RTK-MAC-CorrectionDifferencesReq* field descriptions |
| --- |
| ***master-ReferenceStationID, aux-ReferenceStationList***  These fields specify the Master and Auxiliary Reference Station IDs for which the *GNSS‑RTK‑MAC‑CorrectionDifferences* are requested. |
| ***linkCombinations-PrefList***  This field specifies the dual-frequency combination of L1 and L2 link/frequencies for which the target device wishes to obtain the *GNSS‑RTK‑MAC‑CorrectionDifferences* in the order of preference. The first *GNSS‑Link‑Combinations* in *GNSS-Link-CombinationsList* is the most preferred combination, the second *GNSS‑Link‑Combinations* in *GNSS‑Link‑CombinationsList* is the second most preferred, etc. |

#### *– GNSS-RTK-ResidualsReq*

The IE *GNSS-RTK-ResidualsReq* is used by the target device to request the *GNSS-RTK-Residuals* assistancefrom the location server.

-- ASN1START

GNSS-RTK-ResidualsReq-r15 ::= SEQUENCE {

stationID-r15 GNSS-ReferenceStationID-r15 OPTIONAL,

linkCombinations-PrefList-r15 GNSS-Link-CombinationsList-r15 OPTIONAL,

...

}

-- ASN1STOP

| *GNSS-RTK-ResidualsReq* field descriptions |
| --- |
| ***stationID***  This field specifies the Station ID for which the *GNSS-RTK-Residuals* are requested. |
| ***linkCombinations-PrefList***  This field specifies the dual-frequency combination of L1 and L2 link/frequencies for which the target device wishes to obtain the *GNSS-RTK-Residuals* in the order of preference. The first *GNSS‑Link‑Combinations* in *GNSS‑Link‑CombinationsList* is the most preferred combination, the second *GNSS‑Link‑Combinations* in *GNSS‑Link‑CombinationsList* is the second most preferred, etc. |

#### *– GNSS-RTK-FKP-GradientsReq*

The IE *GNSS-RTK-FKP-GradientsReq* is used by the target device to request the *GNSS-RTK-FKP-Gradients* assistancefrom the location server.

-- ASN1START

GNSS-RTK-FKP-GradientsReq-r15 ::= SEQUENCE {

stationID-r15 GNSS-ReferenceStationID-r15 OPTIONAL,

linkCombinations-PrefList-r15 GNSS-Link-CombinationsList-r15 OPTIONAL,

...

}

-- ASN1STOP

| *GNSS-RTK-FKP-GradientsReq* field descriptions |
| --- |
| ***stationID***  This field specifies the Station ID for which the *GNSS-RTK-FKP-Gradients* are requested. |
| ***linkCombinations-PrefList***  This field specifies the dual-frequency combination of L1 and L2 link/frequencies for which the target device wishes to obtain the *GNSS-RTK-FKP-Gradients* in the order of preference. The first *GNSS‑Link‑Combinations* in *GNSS‑Link‑CombinationsList* is the most preferred combination, the second *GNSS‑Link‑Combinations* in *GNSS‑Link‑CombinationsList* is the second most preferred, etc. |

#### *– GNSS-SSR-OrbitCorrectionsReq*

The IE *GNSS-SSR-OrbitCorrectionsReq* is used by the target device to request the *GNSS-SSR-OrbitCorrections* assistancefrom the location server.

-- ASN1START

GNSS-SSR-OrbitCorrectionsReq-r15 ::= SEQUENCE {

storedNavList-r15 GNSS-NavListInfo-r15 OPTIONAL,

...,

[[

orbit-IntegrityReq-r17 BIT STRING { correlationTimeReq (0)

} (SIZE(1..8)) OPTIONAL

]]

}

-- ASN1STOP

| *GNSS-SSR-OrbitCorrectionsReq* field descriptions |
| --- |
| ***storedNavList***  This list provides information to the location server about which NAV data the target device has currently stored for the particular GNSS indicated by *GNSS-ID*. |
| ***orbit-IntegrityReq***  This field, if present, indicates that the target device requests the IEs *ORBIT-IntegrityParameters* and *SSR-IntegrityOrbitBounds*.  A one‑value at the bit position '0' means that the target device requests the fields *orbitRangeErrorCorrelationTime* and *orbitRangeRateErrorCorrelationTime* in IE *ORBIT-IntegrityParameters*. |

#### *– GNSS-SSR-ClockCorrectionsReq*

The IE *GNSS-SSR-ClockCorrectionsReq* is used by the target device to request the *GNSS-SSR-ClockCorrections* assistancefrom the location server.

-- ASN1START

GNSS-SSR-ClockCorrectionsReq-r15 ::= SEQUENCE {

storedNavList-r15 GNSS-NavListInfo-r15 OPTIONAL,

...,

[[

clock-IntegrityParametersReq-r17 ENUMERATED { true } OPTIONAL,

ssr-IntegrityClockBoundsReq-r17 ENUMERATED { true } OPTIONAL

]]

}

-- ASN1STOP

| *GNSS-SSR-ClockCorrectionsReq* field descriptions |
| --- |
| ***storedNavList***  This list provides information to the location server about which NAV data the target device has currently stored for the particular GNSS indicated by *GNSS-ID*. |
| ***clock-IntegrityParametersReq***  This field, if present, indicates that the target device requests the *CLOCK-IntegrityParameters* in IE *GNSS-SSR-ClockCorrections*. |
| ***ssr-IntegrityClockBoundsReq***  This field, if present, indicates that the target device requests the *SSR-IntegrityClockBounds* in IE *GNSS-SSR-ClockCorrections*. |

#### *– GNSS-SSR-CodeBiasReq*

The IE *GNSS-SSR-CodeBiasReq* is used by the target device to request the *GNSS-SSR-CodeBias* assistancefrom the location server.

-- ASN1START

GNSS-SSR-CodeBiasReq-r15 ::= SEQUENCE {

signal-and-tracking-mode-ID-Map-r15 GNSS-SignalIDs,

storedNavList-r15 GNSS-NavListInfo-r15 OPTIONAL,

...,

[[

ssr-IntegrityCodeBiasBoundsReq-r17 ENUMERATED { requested } OPTIONAL

]]

}

-- ASN1STOP

| *GNSS-SSR-CodeBiasReq* field descriptions |
| --- |
| ***signal-and-tracking-mode-ID-Map***  This field specifies the GNSS signal(s) for which the *GNSS-SSR-CodeBias* is requested. |
| ***storedNavList***  This list provides information to the location server about which NAV data the target device has currently stored for the particular GNSS indicated by *GNSS-ID*. |
| ***ssr-IntegrityCodeBiasBoundsReq***  This field, if present, indicates that the *SSR-IntegrityCodeBiasBounds* are requested. |

#### *– GNSS-SSR-URA-Req*

The IE *GNSS-SSR-URA-Req* is used by the target device to request the *GNSS-SSR-URA* assistancefrom the location server.

-- ASN1START

GNSS-SSR-URA-Req-r16 ::= SEQUENCE {

...

}

-- ASN1STOP

#### *– GNSS-SSR-PhaseBiasReq*

The IE *GNSS-SSR-PhaseBiasReq* is used by the target device to request the *GNSS-SSR-PhaseBias* assistancefrom the location server.

-- ASN1START

GNSS-SSR-PhaseBiasReq-r16 ::= SEQUENCE {

signal-and-tracking-mode-ID-Map-r16 GNSS-SignalIDs,

storedNavList-r16 GNSS-NavListInfo-r15 OPTIONAL,

...,

[[

ssr-IntegrityPhaseBiasBoundsReq-r17 ENUMERATED { requested } OPTIONAL

]]

}

-- ASN1STOP

| *GNSS-SSR-PhaseBiasReq* field descriptions |
| --- |
| ***signal-and-tracking-mode-ID-Map***  This field specifies the GNSS signal(s) for which the *GNSS-SSR-PhaseBias* is requested. |
| ***storedNavList***  This list provides information to the location server about which NAV data the target device has currently stored for the particular GNSS indicated by *GNSS-ID*. |
| ***ssr-IntegrityPhaseBiasBoundsReq***  This field, if present, indicates that the *SSR-IntegrityPhaseBiasBounds* are requested. |

#### *– GNSS-SSR-STEC-CorrectionReq*

The IE *GNSS-SSR-STEC-CorrectionReq* is used by the target device to request the *GNSS-SSR-STEC-Correction* assistancefrom the location server.

-- ASN1START

GNSS-SSR-STEC-CorrectionReq-r16 ::= SEQUENCE {

...,

[[

stec-IntegrityReq-r17 BIT STRING { correlationTimeReq (0)

} (SIZE(1..8)) OPTIONAL

]]

}

-- ASN1STOP

| *GNSS-SSR-STEC-CorrectionReq* field descriptions |
| --- |
| ***stec-IntegrityReq***  This field, if present, indicates that the target device requests the IEs *STEC-IntegrityParameters* and *STEC-IntegrityErrorBounds*.  A one‑value at the bit position '0' means that the target device requests the fields *ionoRangeErrorCorrelationTime* and *ionoRangeRateErrorCorrelationTime* in IE *STEC-IntegrityParameters*. |

#### *– GNSS-SSR-GriddedCorrectionReq*

The IE *GNSS-SSR-GriddedCorrectionReq* is used by the target device to request the *GNSS-SSR-GriddedCorrection* assistancefrom the location server.

-- ASN1START

GNSS-SSR-GriddedCorrectionReq-r16 ::= SEQUENCE {

...,

[[

griddedCorrectionIntegrityReq-r17 ENUMERATED { requested } OPTIONAL

]]

}

-- ASN1STOP

| *GNSS-SSR-GriddedCorrectionReq* field descriptions |
| --- |
| ***griddedCorrectionIntegrityReq***  This field, if present, indicates that the target device requests the IEs *SSR-GriddedCorrectionIntegrityParameters* and *TropoDelayIntegrityErrorBounds*. |

#### – *NavIC-DifferentialCorrectionsReq*

The IE *NavIC-DifferentialCorrectionsReq* is used by the target device to request the NavIC*-DifferentialCorrections* assistance from the location server.

-- ASN1START

NavIC-DifferentialCorrectionsReq-r16 ::= SEQUENCE {

dgnss-SignalsReq-r16 GNSS-SignalIDs,

...

}

-- ASN1STOP

| *NavIC-DifferentialCorrectionsReq* field descriptions |
| --- |
| ***dgnss-SignalsReq***  This field specifies the NavIC Signal(s) for which the *NavIC-DifferentialCorrections* are requested. A one‑value at a bit position means the NavIC differential corrections for the specific signal are requested; a zero‑value means not requested. The target device shall set a maximum of three bits to value 'one'. |

#### – *NavIC-GridModelReq*

The IE *NavIC-GridModelReq* is used by the target device to request the *NavIC-GridModel* assistance from the location server.

-- ASN1START

NavIC-GridModelReq-r16 ::= SEQUENCE {

...

}

-- ASN1STOP

#### *– GNSS-SSR-OrbitCorrectionsSet2Req*

The IE *GNSS-SSR-OrbitCorrectionsSet2Req* is used by the target device to request the *GNSS-SSR-OrbitCorrectionsSet2* assistancefrom the location server.

-- ASN1START

GNSS-SSR-OrbitCorrectionsSet2Req-r17 ::= SEQUENCE {

refEphReq-r17 ENUMERATED { b1c,...},

gnss-SSR-OrbitCorrectionsSet2Req-r17

GNSS-SSR-OrbitCorrectionsReq-r15 OPTIONAL, -- Cond OC2-Req

...

}

-- ASN1STOP

| Conditional presence | Explanation |
| --- | --- |
| *OC2-Req* | The field is mandatory present if the target device requests *GNSS-SSR-OrbitCorrectionsSet2*; otherwise it is not present. |

| *GNSS-SSR-OrbitCorrectionsSet2Req* field descriptions |
| --- |
| ***refEphReq***  This field, if present, indicates that the reference broadcast ephemeris that target device requests the *GNSS-SSR-OrbitCorrectionsSet2* for. |

#### *– GNSS-SSR-ClockCorrectionsSet2Req*

The IE *GNSS-SSR-ClockCorrectionsSet2Req* is used by the target device to request the *GNSS-SSR-ClockCorrectionsSet2* assistancefrom the location server.

-- ASN1START

GNSS-SSR-ClockCorrectionsSet2Req-r17 ::= SEQUENCE {

refEphReq-r17 ENUMERATED { b1c,...},

gnss-SSR-ClockCorrectionsSet2Req-r17

GNSS-SSR-ClockCorrectionsReq-r15 OPTIONAL, -- Cond CC2-Req

...

}

-- ASN1STOP

| Conditional presence | Explanation |
| --- | --- |
| *CC2-Req* | The field is mandatory present if the target device requests *GNSS-SSR-ClockCorrectionsSet2*; otherwise it is not present. |

| *GNSS-SSR-ClockCorrectionsSet2Req* field descriptions |
| --- |
| ***refEphReq***  This field, if present, indicates that the reference broadcast ephemeris that target device requests the *GNSS-SSR-ClockCorrectionsSet2* for. |

#### *– GNSS-SSR-URA-Set2Req*

The IE *GNSS-SSR-URA-Set2Req* is used by the target device to request the *GNSS-SSR-URA-Set2* assistancefrom the location server.

-- ASN1START

GNSS-SSR-URA-Set2Req-r17 ::= SEQUENCE {

refEphReq-r17 ENUMERATED { b1c,...},

...

}

-- ASN1STOP

| *GNSS-SSR-URA-Set2Req* field descriptions |
| --- |
| ***refEphReq***  This field, if present, indicates that the reference broadcast ephemeris that target device requests the *GNSS-SSR-URA-Set2* for. |

#### – *GNSS-LOS-NLOS-GriddedIndicationsReq*

The IE *GNSS-LOS-NLOS-GriddedIndicationsReq* is used by the target device to request the *GNSS-LOS-NLOS-GriddedIndications* assistance from the location server.

-- ASN1START

GNSS-LOS-NLOS-GriddedIndicationsReq-r18 ::= SEQUENCE {

gridPointsSetID-Req-r18 INTEGER (0..16383) OPTIONAL,

relativeLocationInfo-r18 CHOICE {

inside-r18 ENUMERATED {upper-left, upper-right, lower-left, lower-right, ...},

outside-r18 ENUMERATED {north, west, south, east, above, below, ...}

} OPTIONAL, -- Cond Relative

verticalGridType-r18 ENUMERATED {ground-level, threeD},

referenceAltitudeFine-r18 INTEGER (0..9) OPTIONAL,

referenceAltitudeCoarse-r18 INTEGER (-50..900) OPTIONAL,

...

}

-- ASN1STOP

| Conditional presence | Explanation |
| --- | --- |
| *Relative* | This field is mandatory present if a relative position is included in the request. It is absent if the field *gridPointsSetID-Req* is absent. |

#### *– GNSS-SSR-SatellitePCVResidualsReq*

The IE *GNSS-SSR-SatellitePCVResidualsReq* is used by the target device to request the *GNSS-SSR- SatellitePCVResiduals* assistancefrom the location server.

-- ASN1START

GNSS-SSR-SatellitePCVResidualsReq-r18 ::= SEQUENCE {

...

}

-- ASN1STOP

#### 6.5.2.5 GNSS Location Information

#### – *A-GNSS-ProvideLocationInformation*

The IE *A-GNSS-ProvideLocationInformation* is used by the target device to provide location measurements (e.g., pseudo‑ranges, location estimate, velocity) to the location server, together with time information. It may also be used to provide GNSS positioning specific error reason.

-- ASN1START

A-GNSS-ProvideLocationInformation ::= SEQUENCE {

gnss-SignalMeasurementInformation GNSS-SignalMeasurementInformation OPTIONAL,

gnss-LocationInformation GNSS-LocationInformation OPTIONAL,

gnss-Error A-GNSS-Error OPTIONAL,

...

}

-- ASN1STOP

#### 6.5.2.6 GNSS Location Information Elements

#### – *GNSS-SignalMeasurementInformation*

The IE *GNSS-SignalMeasurementInformation* is used by the target device to provide GNSSsignal measurement information to the location server and GNSS‑network time association if requested by the location server. This information includes the measurements of code phase, Doppler, C/No and optionally accumulated carrier phase, also called accumulated deltarange (ADR), which enable the UE‑assisted GNSS method where position is computed in the location server. Figure 6.5.2.6-1 illustrates the relation between some of the fields.

-- ASN1START

GNSS-SignalMeasurementInformation ::= SEQUENCE {

measurementReferenceTime MeasurementReferenceTime,

gnss-MeasurementList GNSS-MeasurementList,

...

}

-- ASN1STOP

| *GNSS-SignalMeasurementInformation* field descriptions |
| --- |
| ***measurementReferenceTime***  This field specifies the GNSS system time for which the information provided in *gnss-MeasurementList* is valid. It may also include network time, if requested by the location server and supported by the target device. |
| ***gnss-MeasurementList***  This fieldprovides GNSS signal measurement information for up to 16 GNSSs. |

#### – *MeasurementReferenceTime*

The IE *MeasurementReferenceTime* is used to specify the time when the measurements provided in *A-GNSS-ProvideLocationInformation* are valid. It may also include GNSS-network time association, in which case reported measurements shall be valid for the cellular frame boundary defined in the network time association.

-- ASN1START

MeasurementReferenceTime ::= SEQUENCE {

gnss-TOD-msec INTEGER (0..3599999),

gnss-TOD-frac INTEGER (0..3999) OPTIONAL,

gnss-TOD-unc INTEGER (0..127) OPTIONAL,

gnss-TimeID GNSS-ID,

networkTime CHOICE {

eUTRA SEQUENCE {

physCellId INTEGER (0..503),

cellGlobalId CellGlobalIdEUTRA-AndUTRA OPTIONAL,

systemFrameNumber BIT STRING (SIZE (10)),

...

},

uTRA SEQUENCE {

mode CHOICE {

fdd SEQUENCE {

primary-CPICH-Info INTEGER (0..511),

...

},

tdd SEQUENCE {

cellParameters INTEGER (0..127),

...

}

},

cellGlobalId CellGlobalIdEUTRA-AndUTRA OPTIONAL,

referenceSystemFrameNumber

INTEGER (0..4095),

...

},

gSM SEQUENCE {

bcchCarrier INTEGER (0..1023),

bsic INTEGER (0..63),

cellGlobalId CellGlobalIdGERAN OPTIONAL,

referenceFrame SEQUENCE {

referenceFN INTEGER (0..65535),

referenceFNMSB INTEGER (0..63) OPTIONAL,

...

},

deltaGNSS-TOD INTEGER (0 .. 127) OPTIONAL,

...

},

...,

nbIoT-r14

SEQUENCE {

nbPhysCellId-r14 INTEGER (0..503),

nbCellGlobalId-r14 ECGI OPTIONAL,

sfn-r14 BIT STRING (SIZE (10)),

hyperSFN-r14 BIT STRING (SIZE (10)) OPTIONAL,

...

},

nr-r15 SEQUENCE {

nrPhysCellId-r15 INTEGER (0..1007),

nrCellGlobalID-r15 NCGI-r15 OPTIONAL,

nr-sfn-r15 BIT STRING (SIZE (10)),

...

}

} OPTIONAL,

...

}

-- ASN1STOP

| *MeasurementReferenceTime* field descriptions |
| --- |
| ***gnss-TOD-msec***  This field specifies the GNSS TOD for which the measurements and/or location estimate are valid. The 22 bits of GNSS TOD are the least significant bits. The most significant bits are derived by the location server to unambiguously derive the GNSS TOD.  The value for GNSS TOD is derived from the GNSS specific system time indicated in *gnss-TimeID* rounded down to the nearest millisecond unit.  Scale factor 1 millisecond. |
| ***gnss-TOD-frac***  This field specifies the fractional part of the GNSS TOD in 250 ns resolution. The total GNSS TOD is given by *gnss-TOD-msec* + *gnss-TOD-frac*.  Scale factor 250 nanoseconds. |
| ***gnss-TOD-unc***  This field provides the accuracy of the relation GNSS-network time when GNSS-network time association is provided. When GNSS-network time association is not provided, this element can be included to provide the accuracy of the reported *gnss-TOD-msec*.  If GNSS TOD is the given GNSS time, then the true GNSS time, corresponding to the provided network time if applicable, as observed at the target device location, lies in the interval [GNSS TOD – *gnss-TOD-unc*, GNSS TOD + *gnss-TOD-unc*].  The uncertainty *r*, expressed in microseconds, is mapped to a number K, with the following formula:  *r* = C\*(((1+x)K)-1)  with C = 0.5 and x = 0.14. To encode any higher value of uncertainty than that corresponding in the above formula to K=127, the same value, K=127, shall also be used. The uncertainty is then coded on 7 bits, as the binary encoding of K. Examples of *gnss-TOD-unc* value are as in the table Value of K to Value of uncertainty relation below.  This field shall be included if the target device provides GNSS-network time relationship. |
| ***gnss-TimeID***  This field specifies the GNSS system time for which the *gnss-TOD-msec* (and *gnss-TOD-frac* if applicable) is provided. |
| ***networkTime***  These fields specify the network time event which the GNSS TOD time stamps.  This field shall be included if the target device provides GNSS-network time relationship. |
| ***physCellId***  This field identifies the reference cell (E-UTRA), as defined in TS 36.331 [12], that is used for the GNSS-network time relation. |
| ***cellGlobalId***  This field specifies the globally unique cell identifier (Evolved Cell Global Identifier (ECGI) in E-UTRA, global UTRAN Cell Identifier in UTRA, or Cell Global Identification (CGI) in GERAN) of the reference cell, as defined in TS 36.331 [12] for E-UTRA and in TS 25.331 [13] for UTRA, for which the GNSS network time relation is provided. |
| ***systemFrameNumber***  This field specifies the system frame number in E-UTRA which the GNSS time time stamps, as defined in TS 36.331 [12]. |
| ***mode***  This field identifies the reference cell for the GNSS-network time relation, as defined in TS 25.331 [13]. |
| ***referenceSystemFrameNumber***  This field specifies the system frame number in UTRA, as defined in TS 25.331 [13], which is used for time stamping. |
| ***bcchCarrier, bsic***  This field identifies the reference cell for the GNSS-network time relation in GERAN, as defined in TS 44.031 [14]. |
| ***referenceFN, referenceFNMSB***  These fields specify the frame number in GERAN which the GNSS time time stamps, as defined in TS 44.031 [14]. The time of the reference frame boundary is as observed by the target device, i.e. without Timing Advance compensation. The *referenceFNMSB* field indicates the most significant bits of the frame number of the reference BTS corresponding to the *GNSS-MeasurementList*. Starting from the complete GSM frame number denoted FN, the target device calculates Reference FN MSB as  Reference FN MSB = floor(FN/42432)  The complete GSM frame number FN can then be reconstructed in the location server by combining the fields *referenceFN* with *referenceFNMSB* in the following way  FN = *referenceFNMSB* \*42432 + *referenceFN* |
| ***deltaGNSS-TOD***  This field specifies the difference in milliseconds between *gnss-TOD-msec*reported and the milli-second part of the SV time tsv\_1 of the first SV in the list reported from the target device, as defined in TS 44.031 [14]. The *deltaGNSS-TOD* is defined as  *deltaGNSS-TOD* = *gnss-TOD-msec* - fix(tsv\_1)  where fix() denotes rounding to the nearest integer towards zero. |
| ***nbPhysCellId***  This field identifies the reference cell, as defined in TS 36.331 [12] that is used for the GNSS-network time relation. |
| ***nbCellGlobalId***  This field specifies the global cell identifier of the NB-IoT reference cell, as defined in TS 36.331 [12], for which the GNSS network time relation is provided. |
| ***sfn***  This field specifies the system frame number in NB-IoT which the GNSS time time stamps, as defined in TS 36.331 [12]. |
| ***hyperSFN***  This field specifies the hyper-SFN in NB-IoT which the GNSS time time stamps, as defined in TS 36.331 [12]. |
| ***nrPhysCellId***  This field identifies the reference cell (NR), as defined in TS 38.331 [35], that is used for the GNSS-network time relation. |
| ***nrCellGlobalID***  This field specifies the NR Cell Global Identifier (NCGI) of the reference cell, as defined in TS 38.331 [35], for which the GNSS network time relation is provided. |
| ***nr-sfn***  This field specifies the system frame number in NR which the GNSS time time stamps, as defined in TS 38.331 [35], |

Value of K to Value of uncertainty relation

|  |  |
| --- | --- |
| **Value of K** | **Value of uncertainty** |
| 0 | 0 microseconds |
| 1 | 0.07 microseconds |
| 2 | 0.1498 microseconds |
| - | - |
| 50 | 349.62 microseconds |
| - | - |
| 127 | ≥ 8430000 microseconds |

#### – *GNSS-MeasurementList*

The IE *GNSS-MeasurementList* is used by the target device to provide measurements of code phase, Doppler, C/No and optionally accumulated carrier phase, also called accumulated deltarange (ADR).

-- ASN1START

GNSS-MeasurementList ::= SEQUENCE (SIZE(1..16)) OF GNSS-MeasurementForOneGNSS

GNSS-MeasurementForOneGNSS ::= SEQUENCE {

gnss-ID GNSS-ID,

gnss-SgnMeasList GNSS-SgnMeasList,

...

}

GNSS-SgnMeasList ::= SEQUENCE (SIZE(1..8)) OF GNSS-SgnMeasElement

GNSS-SgnMeasElement ::= SEQUENCE {

gnss-SignalID GNSS-SignalID,

gnss-CodePhaseAmbiguity INTEGER (0..127) OPTIONAL,

gnss-SatMeasList GNSS-SatMeasList,

...

}

GNSS-SatMeasList ::= SEQUENCE (SIZE(1..64)) OF GNSS-SatMeasElement

GNSS-SatMeasElement ::= SEQUENCE {

svID SV-ID,

cNo INTEGER (0..63),

mpathDet ENUMERATED {notMeasured (0), low (1), medium (2), high (3), ...},

carrierQualityInd INTEGER (0..3) OPTIONAL,

codePhase INTEGER (0..2097151),

integerCodePhase INTEGER (0..127) OPTIONAL,

codePhaseRMSError INTEGER (0..63),

doppler INTEGER (-32768..32767) OPTIONAL,

adr INTEGER (0..33554431) OPTIONAL,

...,

[[

adrMSB-r15 INTEGER (0..15) OPTIONAL,

adrSign-r15 ENUMERATED {positive, negative} OPTIONAL,

adrRMSerror-r15 INTEGER (0..127) OPTIONAL,

delta-codePhase-r15 INTEGER (0..7) OPTIONAL

]]

}

-- ASN1STOP

| *GNSS-MeasurementList* field descriptions |
| --- |
| ***gnss-ID***  This field identifies the GNSS constellation on which the GNSS signal measurements were measured. Measurement information for up to 16 GNSSs can be included. |
| ***gnss-SgnMeasList***  This list provides GNSS signal measurement information for up to 8 GNSS signal types per GNSS. |
| ***gnss-SignalID***  This field identifies the signal on which GNSS signal measurement parameters were measured. |
| ***gnss-CodePhaseAmbiguity***  This field provides the ambiguity of the code phase measurement. It is given in units of milli-seconds in the range between between 0 and 127 milli-seconds.  The total code phase for a satellite k (Satk) is given modulo this *gnss-CodePhaseAmbiguity* and is reconstructed with:  Code\_Phase\_Tot(Satk) = *codePhase*(Satk) + *integerCodePhase*(Satk) + n \* *gnss-CodePhaseAmbiguity*, n= 0,1,2,...  If there is no code phase ambiguity, the *gnss-CodePhaseAmbiguity* shall be set to 0.  The field is optional. If *gnss-CodePhaseAmbiguity* is absent, the default value is 1 milli-second. |
| ***gnss-SatMeasList***  This list provides GNSS signal measurement information for up to 64 GNSS satellites. |
| ***svID***  This field identifies the satellite on which the GNSS signal measurements were measured. |
| ***cNo***  This field provides an estimate of the carrier‑to‑noise ratio of the received signal from the particular satellite. The target device shall set this field to the value of the satellite C/N0, as referenced to the antenna connector, in units of 1 dB‑Hz, in the range from 0 to 63 dB‑Hz.  Scale factor 1 dB‑Hz. |
| ***mpathDet***  This field contains the multipath indicator value, defined in the table Value of *mpathDet* to Multipath Indication relation below. |
| ***carrierQualityInd***  If the fields *adrMSB*, *adrSign*, *adrRMSerror*, and *delta-codePhase* are not present:  This field indicates the quality of a carrier phase measurement. The LSB indicates the data polarity, that is, if the data from a specific satellite is received inverted, this is indicated by setting the LSB value to '1'. In the case the data is not inverted, the LSB is set to '0'. The MSB indicates if accumulation of the carrier phase has been continuous, that is, without cycle slips since the previous measurement report. If the carrier phase accumulation has been continuous, the MSB value is set to '1X'. Otherwise, the MSB is set to '0X'.  This field is optional but shall be included if the *adr* field is included. See table Bit to Polarity Indication relation below.  If any of the fields *adrMSB*, *adrSign*, *adrRMSerror*, or *delta-codePhase* are present:  This field indicates the quality of a carrier phase measurement. The LSB indicates the half-cycle ambiguity, that is, if there are no half-cycle ambiguities present in the ADR measurement report the LSB is set to '0'. In the case there are half-cycle ambiguities present in the ADR measurement report the LSB is set to '1'. When reporting ADR with unresolved polarity encoding the target device shall set this bit to 1.  The MSB indicates if accumulation of the carrier phase has been continuous, that is, without cycle slips since the previous measurement report. If the carrier phase accumulation has been continuous (no cycle slips), the MSB value is set to '1X'. Otherwise, the MSB is set to '0X'. If polarity resolution forced the ADR measurement to be corrected by half-a-cycle, then the MSB must be set to '0', indicating that despite continuous tracking the reported ADR experienced non-continuity. See table Bit to Ambiguity Indication relation below.  The target device shall include this field if the *adr* field is included. |
| ***codePhase***  This field contains the whole and fractional value of the code-phase measurement made by the target device for the particular satellite signal at the time of measurement in the units of ms. GNSS specific code phase measurements (e.g. chips) are converted into unit of ms by dividing the measurements by the nominal values of the measured signal chipping rate.  Scale factor 2-21 milli‑seconds, in the range from 0 to (1-2-21) milli‑seconds. |
| ***integerCodePhase***  This field indicates the integer milli‑second part of the code phase that is expressed modulo the *gnss-CodePhaseAmbiguity*. The value of the ambiguity is given in the *gnss-CodePhaseAmbiguity* field.  The *integerCodePhase*is optional. If *integerCodePhase* is absent, the default value is 0 milli-second.  Scale factor 1 milli-second, in the range from 0 to 127 milli‑seconds. |
| ***codePhaseRMSError***  This field contains the pseudorange RMS error value. This parameter is specified according to a floating-point representation shown in the table below. |
| ***doppler***  This field contains the Doppler measured by the target device for the particular satellite signal. This information can be used to compute the 3-D velocity of the target device. Doppler measurements are converted into unit of m/s by multiplying the Doppler measurement in Hz by the nominal wavelength of the measured signal.  Scale factor 0.04 metre/second. This field is optional, but shall be included, if the *velocityRequest* in *CommonIEsRequestLocationInformation* is set to TRUE. |
| ***adr***  This field contains the absolute value of the ADR measurement measured by the target device for the particular satellite signal. This information can be used to compute the 3-D velocity or high-accuracy position of the target device. ADR measurements are converted into units of metre by multiplying the ADR measurement by the nominal wavelength of the measured signal.  Scale factor 2-10 metres, in the range from 0 to 32767.5 metres. This field is optional, but shall be included, if the *adrMeasReq* in *GNSS-PositioningInstructions* is set to TRUE and if ADR measurements are supported by the target device (i.e., *adr-Support* is set to TRUE in *A-GNSS-ProvideCapabilities*). |
| ***adrMSB***  This field contains the 4-MSBs of the ADR measurement in the case the ADR measurement is outside the range of the field *adr* alone. Scale factor 32768 metres.  If present, the full ADR measurement is constructed as *adrMSB* × 32768 + *adr* × 2-10 metres, representing measurements in the range from 0 to 524287.9990234375 metres.  This field is optional, but shall be included, if the capability *adrEnhancementsSupport* is set to TRUE and the ADR measurement is outside the range of the *adr* field. |
| ***adrSign***  This field indicates the sign of the ADR measurement. |
| ***adrRMSerror***  This field contains the ADR root mean squared error value. Scale factor 2-10 metres. |
| ***delta-codePhase***  This field specifies the higher resolution of the *codePhase* measurement. Scale factor 2-24 milli‑seconds.  The full code phase measurement is constructed as *codePhase* × 2-21 + *delta-codePhase* × 2-24 milli-seconds, in the range from 0 to (1-2-24) milli‑seconds. |

Value of *mpathDet* to Multipath Indication relation

|  |  |
| --- | --- |
| Value of *mpathDet* | Multipath Indication |
| 00 | Not measured |
| 01 | Low, MP error < 5m |
| 10 | Medium, 5m < MP error < 43m |
| 11 | High, MP error > 43m |

Bit to Polarity Indication relation

|  |  |
| --- | --- |
| Value | Polarity Indication |
| 0 | Data Direct, carrier phase not continuous |
| 1 | Data Inverted, carrier phase not continuous |
| 2 | Data Direct, carrier phase continuous |
| 3 | Data Inverted, carrier phase continuous |

Bit to Ambiguity Indication relation

|  |  |  |
| --- | --- | --- |
| Value | Value MSB, LSB | Polarity Indication |
| 0 | 00 | carrier phase not continuous, no half-cycle ambiguity |
| 1 | 01 | carrier phase not continuous, half-cycle ambiguity |
| 2 | 10 | carrier phase continuous, no half-cycle ambiguity |
| 3 | 11 | carrier phase continuous, half-cycle ambiguity |

floating-point representation

| Index | Mantissa | Exponent | Floating-Point value, xi | Pseudorange value, P |
| --- | --- | --- | --- | --- |
| 0 | 000 | 000 | 0.5 | P < 0.5 |
| 1 | 001 | 000 | 0.5625 | 0.5 <= P < 0.5625 |
| I | x | y | 0.5 \* (1 + x/8) \* 2y | xi-1 <= P < xi |
| 62 | 110 | 111 | 112 | 104 <= P < 112 |
| 63 | 111 | 111 | -- | 112 <= P |



Figure 6.5.2.6-1: Exemplary calculation of some GNSS Signal Measurement Information fields.

#### – *GNSS-LocationInformation*

The IE *GNSS-LocationInformation* is included by the target device when location and optionally velocity information derived using GNSS or hybrid GNSS and other measurements is provided to the location server.

-- ASN1START

GNSS-LocationInformation ::= SEQUENCE {

measurementReferenceTime MeasurementReferenceTime,

agnss-List GNSS-ID-Bitmap,

...,

[[

ha-GNSS-Metrics-r17 HA-GNSS-Metrics-r17 OPTIONAL

]]

}

-- ASN1STOP

| *GNSS-LocationInformation* field descriptions |
| --- |
| ***measurementReferenceTime***  This field specifies the GNSS system time for which the location estimate and optionally velocity are valid. It may also include GNSS-network time relationship, if requested by the location server and supported by the target device. |
| ***agnss-List***  This fieldprovides a list of satellite systems used by the target device to calculate the location estimate and velocity estimate, if included. This is represented by a bit string in *GNSS-ID-Bitmap*, with a one‑value at the bit position means the particular method has been used; a zero‑value means not used. |
| ***ha-GNSS-Metrics***  This fieldprovides high accuracy GNSS positioning metrics associated to the reported location estimate. |

#### *– HA-GNSS-Metrics*

The IE *HA-GNSS-Metrics* is included by the target device when high accuracy GNSS positioning metrics associated to a location estimate is provided to the location server. The parameters provided in IE *HA-GNSS-Metrics* are used as specified for sentence type GGA in [51] and apply to all GNSSs and types of high accuracy GNSS assistance data.

-- ASN1START

HA-GNSS-Metrics-r17 ::= SEQUENCE {

nrOfUsedSatellites-r17 INTEGER (0..64),

hdopi-r17 INTEGER (1..256) OPTIONAL,

pdopi-r17 INTEGER (1..256) OPTIONAL,

age-r17 INTEGER (0..99) OPTIONAL,

fixType-r17 ENUMERATED {carrier-phase-float,

carrier-phase-fix, ...} OPTIONAL,

...

}

-- ASN1STOP

| *HA-GNSS-Metrics* field descriptions |
| --- |
| ***nrOfUsedSatellites***  This field specifies number of used GNSS satellites for the location estimate provided by the target device. |
| ***hdopi***  This field specifies the horizontal dilution of precision for the location estimate, scale factor 0.1. |
| ***pdopi***  This field specifies the 3D position dilution of precision, scale factor 0.1. |
| ***age***  This field, if supported by the device, specifies the age of the most recent used assistance data for high accuracy GNSS, scale factor 0.1 second. |
| ***fixType***  This field specifies the positioning fix type, based on the positioning fix quality indicators RTK float and RTK fix of [51]. Specifically:  *- carrier-phase-float* - converged carrier phase floating point ambiguity resolution  *- carrier-phase-fix* - converging carrier phase integer ambiguity resolution |

#### 6.5.2.7 GNSS Location Information Request

#### – *A-GNSS-RequestLocationInformation*

The IE *A-GNSS-RequestLocationInformation* is used by the location server to request location information from the target device using GNSS.

-- ASN1START

A-GNSS-RequestLocationInformation ::= SEQUENCE {

gnss-PositioningInstructions GNSS-PositioningInstructions,

...

}

-- ASN1STOP

#### 6.5.2.8 GNSS Location Information Request Elements

#### – *GNSS-PositioningInstructions*

The IE *GNSS-PositioningInstructions* is used to provide GNSS measurement instructions.

-- ASN1START

GNSS-PositioningInstructions ::= SEQUENCE {

gnss-Methods GNSS-ID-Bitmap,

fineTimeAssistanceMeasReq BOOLEAN,

adrMeasReq BOOLEAN,

multiFreqMeasReq BOOLEAN,

assistanceAvailability BOOLEAN,

...,

[[

ha-GNSS-Req-r15 ENUMERATED { true } OPTIONAL -- Cond UEB

]],

[[

ha-GNSS-MetricsReq-r17 ENUMERATED { true } OPTIONAL -- Cond UEB

]]

}

-- ASN1STOP

| **Conditional presence** | **Explanation** |
| --- | --- |
| *UEB* | The field is optionally present, need OP, if the *locationInformationType* is set to *locationEstimateRequired, locationEstimatePreferred, or* *locationMeasurementsPreferred*; oltherwise it is not present. |

| *GNSS-PositioningInstructions* field descriptions |
| --- |
| ***gnssMethods***  This field indicates the satellite systems allowed by the location server. This is represented by a bit string in *GNSS-ID-Bitmap*, with a one‑value at the bit position means the particular GNSS is allowed; a zero‑value means not allowed. The target device shall not request assistance data or report or obtain measurements for systems that are not indicated in this bit map. At least one of the bits in this bit map shall be set to value one. |
| ***fineTimeAssistanceMeasReq***  This field indicates whether the target device is requested to report GNSS-network time association. TRUE means requested. |
| ***adrMeasReq***  This field indicates whether the target device is requested to include ADR measurements in *GNSS-MeasurementList* IE or not. TRUE means requested. |
| ***multiFreqMeasReq***  This field indicates whether the target device is requested to report measurements on multiple supported GNSS signal types in *GNSS-MeasurementList* IE or not. TRUE means requested. |
| ***assistanceAvailability***  This field indicates whether the target device may request additional GNSS assistance data from the server. TRUE means allowed and FALSE means not allowed. |
| ***ha-GNSS-Req***  This field, if present, indicates that any location estimate provided by the target device should be obtained using high accuracy RTK/PPP methods. |
| ***ha-GNSS-MetricsReq***  This field, if present, indicates that any location estimate provided by the target device should be reported with high accuracy GNSS positioning metrics. |

#### 6.5.2.9 GNSS Capability Information

#### – *A-GNSS-ProvideCapabilities*

The IE *A-GNSS-Provide-Capabilities* is used by the target device to indicate its capability to support A-GNSS and to provide its A-GNSS location capabilities (e.g., GNSSs and assistance data supported) to the location server.

-- ASN1START

A-GNSS-ProvideCapabilities ::= SEQUENCE {

gnss-SupportList GNSS-SupportList OPTIONAL,

assistanceDataSupportList AssistanceDataSupportList OPTIONAL,

locationCoordinateTypes LocationCoordinateTypes OPTIONAL,

velocityTypes VelocityTypes OPTIONAL,

...,

[[ periodicalReportingNotSupported-r14

PositioningModes OPTIONAL,

idleStateForMeasurements-r14

ENUMERATED { required } OPTIONAL

]],

[[ periodicAssistanceData-r15

BIT STRING { solicited (0),

unsolicited (1) } (SIZE (1..8)) OPTIONAL

]],

[[ scheduledLocationRequestSupported-r17

ScheduledLocationTimeSupportPerMode-r17 OPTIONAL

]],

[[ periodicReportingIntervalMsSupport-r18

PeriodicReportingIntervalMsSupportPerMode-r18 OPTIONAL

]]

}

GNSS-SupportList ::= SEQUENCE (SIZE(1..16)) OF GNSS-SupportElement

GNSS-SupportElement ::= SEQUENCE {

gnss-ID GNSS-ID,

sbas-IDs SBAS-IDs OPTIONAL, -- Cond GNSS-ID-SBAS

agnss-Modes PositioningModes,

gnss-Signals GNSS-SignalIDs,

fta-MeasSupport SEQUENCE {

cellTime AccessTypes,

mode PositioningModes,

...

} OPTIONAL, -- Cond fta

adr-Support BOOLEAN,

velocityMeasurementSupport BOOLEAN,

...,

[[

adrEnhancementsSupport-r15 ENUMERATED { true } OPTIONAL,

ha-gnss-Modes-r15 PositioningModes OPTIONAL

]],

[[

ha-gnss-MetricsSupport-r17 ENUMERATED { true } OPTIONAL

]]

}

AssistanceDataSupportList ::= SEQUENCE {

gnss-CommonAssistanceDataSupport GNSS-CommonAssistanceDataSupport,

gnss-GenericAssistanceDataSupport GNSS-GenericAssistanceDataSupport,

...

}

-- ASN1STOP

| Conditional presence | Explanation |
| --- | --- |
| *GNSS‑ID‑SBAS* | The field is mandatory present if the *GNSS‑ID* = *sbas*; otherwise it is not present. |
| *fta* | The field is mandatory present if the target device supports the reporting of fine time assistance measurements; otherwise it is not present. |

| *A-GNSS-ProvideCapabilities* field descriptions |
| --- |
| ***gnss-SupportList***  This field specifies the list of GNSS supported by the target device and the target device capabilities associated with each of the supported GNSS. This field shall be present if the *gnss-SupportListReq* in the A-GNSS *-RequestCapabilities* IE is set to TRUE and if the target device supports the A-GNSS positioning method. If the IE *A-GNSS-Provide-Capabilities* is provided unsolicited, this field shall be included if the target device supports the assisted GNSS positioning method. |
| ***gnss-ID***  This field specifies the GNSS supported by the target device for which the capabilities in *GNSS-SupportElement* are provided. |
| ***sbas-IDs***  This field specifies the SBAS(s) supported by the target device. This is represented by a bit string, with a one‑value at the bit position means the particular SBAS is supported; a zero‑value means not supported. |
| ***agnss-Modes***  This field specifies the GNSS mode(s) supported by the target device for the GNSS indicated by *gnss-ID*. This is represented by a bit string, with a one‑value at the bit position means the particular GNSS mode is supported; a zero‑value means not supported. |
| ***gnss-Signals***  This field specifies the GNSS signal(s) supported by the target device for the GNSS indicated by *gnss-ID*. This is represented by a bit string, with a one‑value at the bit position means the particular GNSS signal type is supported; a zero‑value means not supported. |
| ***fta-MeasSupport***  This field specifies that the target device is capable of performing fine time assistance measurements (i.e., GNSS‑cellular time association reporting). The *cellTime* field specifies for which cellular network(s) this capability is supported. This is represented by a bit string, with a one‑value at the bit position means FTA measurements for the specific cellular network time is supported; a zero‑value means not supported. The *mode* field specifies for which GNSS mode(s) FTA measurements are supported by the target device. This is represented by a bit string, with a one‑value at the bit position means FTA measurements for the GNSS mode is supported; a zero‑value means not supported. |
| ***adr-Support***  This field specifies whether the target device supports ADR measurement reporting. TRUE means supported. |
| ***velocityMeasurementSupport***  This field specifies whether the target device supports measurement reporting related to velocity. TRUE means supported. |
| ***assistanceDataSupportList***  This list defines the assistance data and assistance data choices supported by the target device. This field shall be present if the *assistanceDataSupportListReq* in the A-GNSS*-RequestCapabilities* IE is set to TRUE and if the target device supports GNSS assistance data. If the IE *A-GNSS-Provide-Capabilities* is provided unsolicited, this field shall be included if the target device supports any GNSS assistance data. |
| ***locationCoordinateTypes***  This parameter identifies the geographical location coordinate types that a target device supports for GNSS. TRUE indicates that a location coordinate type is supported and FALSE that it is not. This field shall be present if the *locationVelocityTypesReq* in the A-GNSS*-RequestCapabilities* IE is set to TRUE and if the target device supports UE-based or standalone GNSS positioning method. If the IE *A-GNSS-Provide-Capabilities* is provided unsolicited, this field shall be included if the target device supports UE-based or standalone GNSS positioning method. |
| ***velocityTypes***  This parameter identifies the velocity types that a target device supports for GNSS. TRUE indicates that a velocity type is supported and FALSE that it is not. FALSE for all velocity types indicates that velocity reporting is not supported. This field shall be present if the *locationVelocityTypesReq* in the A-GNSS*-RequestCapabilities* IE is set to TRUE and if the target device supports UE-based or standalone GNSS positioning method. If the IE *A-GNSS-Provide-Capabilities* is provided unsolicited, this field shall be included if the target device supports UE-based or standalone GNSS positioning method. |
| ***periodicalReportingNotSupported***  This field, if present, specifies the positioning modes for which the target device does not support *periodicalReporting.* This is represented by a bit string, with a one‑value at the bit position means *periodicalReporting* for the positioning mode is not supported; a zero‑value means supported. If this field is absent, the location server may assume that the target device supports *periodicalReporting* in *CommonIEsRequestLocationInformation* for each supported positioning mode. |
| ***idleStateForMeasurements***  This field, if present, indicates that the target device requires idle state to perform GNSS measurements. |
| ***periodicAssistanceData***  This field identifies the periodic assistance data delivery procedures supported by the target device. This is represented by a bit string, with a one value at the bit position means the periodic assistance data delivery procedure is supported; a zero value means not supported. Bit 0 (solicited) represents the procedure according to clause 5.2.1a; bit (1) (unsolicited) represents the procedure according to clause 5.2.2a. |
| ***adrEnhancementsSupport***  This field, if present, indicates that the target device supports the fields *adrMSB*, *adrSign*, *adrRMSerror*, and *delta‑codePhase* in IE *GNSS-MeasurementList*.  This field may only be present if *adr-Support* is set to TRUE, and shall be absent if *adr-Support* is set to FALSE. |
| ***ha-gnss-Modes***  This field specifies the High-Accuracy GNSS mode(s) supported by the target device for the GNSS indicated by *gnss‑ID*. This is represented by a bit string, with a one‑value at the bit position means the particular GNSS mode is supported; a zero‑value means not supported. |
| ***ha-gnss-MetricsSupport***  This field specifies that high accuracy GNSS positioning metrics are supported by the target device. |
| ***scheduledLocationRequestSupported***  This field, if present, specifies the positioning modes for which the target device supports scheduled location requests – i.e., supports the IE *ScheduledLocationTime* in IE *CommonIEsRequestLocationInformation* – and the time base(s) supported for the scheduled location time for each positioning mode. If this field is absent, the target device does not support scheduled location requests. |
| ***periodicReportingIntervalMsSupport***  This field, if present, specified the supported minimum millisecond periodic reporting interval for location information per positioning mode – i.e., supports the subfield *reportingIntervalMs* of the IE *PeriodicalReportingCriteriaExt* in IE *CommonIEsRequestLocationInformation* – and the minimum millisecond report interval supported for the periodic reporting. |

#### 6.5.2.10 GNSS Capability Information Elements

#### – *GNSS-CommonAssistanceDataSupport*

The IE *GNSS-CommonAssistanceDataSupport* is used by the target device to provide information on supported GNSS common assistance data types to the location server.

-- ASN1START

GNSS-CommonAssistanceDataSupport ::= SEQUENCE {

gnss-ReferenceTimeSupport GNSS-ReferenceTimeSupport

OPTIONAL, -- Cond RefTimeSup

gnss-ReferenceLocationSupport GNSS-ReferenceLocationSupport

OPTIONAL, -- Cond RefLocSup

gnss-IonosphericModelSupport GNSS-IonosphericModelSupport

OPTIONAL, -- Cond IonoModSup

gnss-EarthOrientationParametersSupport GNSS-EarthOrientationParametersSupport

OPTIONAL, -- Cond EOPSup

...,

[[

gnss-RTK-ReferenceStationInfoSupport-r15

GNSS-RTK-ReferenceStationInfoSupport-r15

OPTIONAL, -- Cond ARPSup

gnss-RTK-AuxiliaryStationDataSupport-r15

GNSS-RTK-AuxiliaryStationDataSupport-r15

OPTIONAL -- Cond AuxARPSup

]],

[[

gnss-Integrity-ServiceParametersSupport-r17

GNSS-Integrity-ServiceParametersSupport-r17

OPTIONAL, -- Cond IntServiceSup

gnss-Integrity-ServiceAlertSupport-r17

GNSS-Integrity-ServiceAlertSupport-r17

OPTIONAL -- Cond IntAlertSup

]],

[[

gnss-SSR-IOD-UpdateSupport-r18 GNSS-SSR-IOD-UpdateSupport-r18

OPTIONAL -- Cond IODUpdateSup

]]

}

-- ASN1STOP

| Conditional presence | Explanation |
| --- | --- |
| *RefTimeSup* | The field is mandatory present if the target device supports *GNSS-ReferenceTime*; otherwise it is not present. |
| *RefLocSup* | This field is mandatory present if the target device supports *GNSS-ReferenceLocation*; otherwise it is not present. |
| *IonoModSup* | This field is mandatory present if the target device supports *GNSS-IonosphericModel*; otherwise it is not present. |
| *EOPSup* | This field is mandatory present if the target device supports *GNSS-EarthOrientationParameters*; otherwise it is not present. |
| *ARPSup* | This field is mandatory present if the target device supports *GNSS‑RTK‑ReferenceStationInfo*; otherwise it is not present. |
| *AuxARPSup* | This field is mandatory present if the target device supports *GNSS‑RTK‑AuxiliaryStationData*; otherwise it is not present. |
| *IntServiceSup* | This field is mandatory present if the target device supports *GNSS-Integrity-ServiceParameters*; otherwise it is not present. |
| *IntAlertSup* | This field is mandatory present if the target device supports *GNSS-Integrity-ServiceAlert*; otherwise it is not present. |
| *IODUpdateSup* | This field is mandatory present if the target device supports *GNSS SSR-IOD-Update*; otherwise it is not present. |

#### – *GNSS-ReferenceTimeSupport*

-- ASN1START

GNSS-ReferenceTimeSupport ::= SEQUENCE {

gnss-SystemTime GNSS-ID-Bitmap,

fta-Support AccessTypes OPTIONAL, -- Cond fta

...

}

-- ASN1STOP

| Conditional presence | Explanation |
| --- | --- |
| *fta* | The field is mandatory present if the target device supports fine time assistance in *GNSSReferenceTime* IE; otherwise it is not present. |

| *GNSS-ReferenceTimeSupport* field descriptions |
| --- |
| ***gnss-SystemTime***  This field specifies the GNSS system time(s) supported by the target device. This is represented by a bit string in *GNSS-ID-Bitmap*, with a one‑value at the bit position means the particular GNSS system time is supported; a zero‑value means not supported. |
| ***fta-Support***  This field specifies that the target device supports fine time assistance (i.e., GNSS‑cellular time association) in *GNSS-ReferenceTime* IE. This is represented by a bit string in *AccessTypes*, with a one‑value at the bit position means FTA for the specific cellular network time is supported; a zero‑value means not supported. |

#### – *GNSS-ReferenceLocationSupport*

-- ASN1START

GNSS-ReferenceLocationSupport ::= SEQUENCE {

...

}

-- ASN1STOP

#### – *GNSS-IonosphericModelSupport*

-- ASN1START

GNSS-IonosphericModelSupport ::= SEQUENCE {

ionoModel BIT STRING { klobuchar (0),

neQuick (1),

klobuchar2-r16 (2) } (SIZE (1..8)),

...

}

-- ASN1STOP

| *GNSS-IonosphericModelSupport* field descriptions |
| --- |
| ***ionoModel***  This field specifies the ionospheric model(s) supported by the target device. This is represented by a bit string, with a one‑value at the bit position means the particular ionospheric model is supported; a zero‑value means not supported. |

#### – *GNSS-EarthOrientationParametersSupport*

-- ASN1START

GNSS-EarthOrientationParametersSupport ::= SEQUENCE {

...

}

-- ASN1STOP

#### – *GNSS-RTK-ReferenceStationInfoSupport*

-- ASN1START

GNSS-RTK-ReferenceStationInfoSupport-r15 ::= SEQUENCE {

...

}

-- ASN1STOP

#### – *GNSS-RTK-AuxiliaryStationDataSupport*

-- ASN1START

GNSS-RTK-AuxiliaryStationDataSupport-r15 ::= SEQUENCE {

...

}

-- ASN1STOP

#### – *GNSS-Integrity-ServiceParametersSupport*

-- ASN1START

GNSS-Integrity-ServiceParametersSupport-r17 ::= SEQUENCE {

...

}

-- ASN1STOP

#### – *GNSS-Integrity-ServiceAlertSupport*

-- ASN1START

GNSS-Integrity-ServiceAlertSupport-r17 ::= SEQUENCE {

...

}

-- ASN1STOP

#### – *GNSS-SSR-IOD-UpdateSupport*

-- ASN1START

GNSS-SSR-IOD-UpdateSupport-r18 ::= SEQUENCE {

...

}

-- ASN1STOP

#### – *GNSS-GenericAssistanceDataSupport*

The IE *GNSS-GenericAssistanceDataSupport* is used by the target device to provide information on supported GNSS generic assistance data types to the location server for each supported GNSS.

-- ASN1START

GNSS-GenericAssistanceDataSupport ::=

SEQUENCE (SIZE (1..16)) OF GNSS-GenericAssistDataSupportElement

GNSS-GenericAssistDataSupportElement ::= SEQUENCE {

gnss-ID GNSS-ID,

sbas-ID SBAS-ID OPTIONAL, -- Cond GNSS‑ID‑SBAS

gnss-TimeModelsSupport GNSS-TimeModelListSupport

OPTIONAL, -- Cond TimeModSup

gnss-DifferentialCorrectionsSupport GNSS-DifferentialCorrectionsSupport

OPTIONAL, -- Cond DGNSS-Sup

gnss-NavigationModelSupport GNSS-NavigationModelSupport

OPTIONAL, -- Cond NavModSup

gnss-RealTimeIntegritySupport GNSS-RealTimeIntegritySupport

OPTIONAL, -- Cond RTISup

gnss-DataBitAssistanceSupport GNSS-DataBitAssistanceSupport

OPTIONAL, -- Cond DataBitsSup

gnss-AcquisitionAssistanceSupport GNSS-AcquisitionAssistanceSupport

OPTIONAL, -- Cond AcquAssistSup

gnss-AlmanacSupport GNSS-AlmanacSupport

OPTIONAL, -- Cond AlmanacSup

gnss-UTC-ModelSupport GNSS-UTC-ModelSupport

OPTIONAL, -- Cond UTCModSup

gnss-AuxiliaryInformationSupport GNSS-AuxiliaryInformationSupport

OPTIONAL, -- Cond AuxInfoSup

...,

[[

bds-DifferentialCorrectionsSupport-r12

BDS-DifferentialCorrectionsSupport-r12

OPTIONAL, -- Cond DBDS-Sup

bds-GridModelSupport-r12 BDS-GridModelSupport-r12

OPTIONAL -- Cond BDS-GridModSup

]],

[[

gnss-RTK-ObservationsSupport-r15

GNSS-RTK-ObservationsSupport-r15

OPTIONAL, -- Cond RTK-OSR-Sup

glo-RTK-BiasInformationSupport-r15

GLO-RTK-BiasInformationSupport-r15

OPTIONAL, -- Cond GLO-CPB-Sup

gnss-RTK-MAC-CorrectionDifferencesSupport-r15

GNSS-RTK-MAC-CorrectionDifferencesSupport-r15

OPTIONAL, -- Cond MAC-Sup

gnss-RTK-ResidualsSupport-r15 GNSS-RTK-ResidualsSupport-r15

OPTIONAL, -- Cond Res-Sup

gnss-RTK-FKP-GradientsSupport-r15

GNSS-RTK-FKP-GradientsSupport-r15

OPTIONAL, -- Cond FKP-Sup

gnss-SSR-OrbitCorrectionsSupport-r15

GNSS-SSR-OrbitCorrectionsSupport-r15

OPTIONAL, -- Cond OC-Sup

gnss-SSR-ClockCorrectionsSupport-r15

GNSS-SSR-ClockCorrectionsSupport-r15

OPTIONAL, -- Cond CC-Sup

gnss-SSR-CodeBiasSupport-r15 GNSS-SSR-CodeBiasSupport-r15

OPTIONAL -- Cond CB-Sup

]],

[[

gnss-SSR-URA-Support-r16 GNSS-SSR-URA-Support-r16 OPTIONAL, -- Cond URA-Sup

gnss-SSR-PhaseBiasSupport-r16 GNSS-SSR-PhaseBiasSupport-r16

OPTIONAL, -- Cond PB-Sup

gnss-SSR-STEC-CorrectionSupport-r16

GNSS-SSR-STEC-CorrectionSupport-r16

OPTIONAL, -- Cond STEC-Sup

gnss-SSR-GriddedCorrectionSupport-r16

GNSS-SSR-GriddedCorrectionSupport-r16

OPTIONAL, -- Cond Grid-Sup

navic-DifferentialCorrectionsSupport-r16

NavIC-DifferentialCorrectionsSupport-r16

OPTIONAL, -- Cond DNavIC-Sup

navic-GridModelSupport-r16 NavIC-GridModelSupport-r16

OPTIONAL -- Cond NavIC-GridModSup

]],

[[

gnss-SSR-OrbitCorrectionsSet2Support-r17

GNSS-SSR-OrbitCorrectionsSet2Support-r17

OPTIONAL, -- Cond OC2-Sup

gnss-SSR-ClockCorrectionsSet2Support-r17

GNSS-SSR-ClockCorrectionsSet2Support-r17

OPTIONAL, -- Cond CC2-Sup

gnss-SSR-URA-Set2Support-r17 GNSS-SSR-URA-Set2Support-r17

OPTIONAL -- Cond URA2-Sup

]],

[[

gnss-LOS-NLOS-GriddedIndicationsSupport-r18

GNSS-LOS-NLOS-GriddedIndicationsSupport-r18

OPTIONAL, -- Cond LOS-NLOS-Grid-Sup

gnss-SSR-SatellitePCVResidualsSupport-r18

GNSS-SSR-SatellitePCVResidualsSupport-r18

OPTIONAL -- Cond SatPCV-Sup

]]

}

-- ASN1STOP

| Conditional presence | Explanation |
| --- | --- |
| *GNSS‑ID‑SBAS* | The field is mandatory present if the *GNSS‑ID* = *sbas*; otherwise it is not present. |
| *TimeModSup* | The field is mandatory present if the target device supports *GNSS-TimeModelList*; otherwise it is not present. |
| *DGNSS-Sup* | The field is mandatory present if the target device supports *GNSS-DifferentialCorrections*; otherwise it is not present. |
| *NavModSup* | The field is mandatory present if the target device supports *GNSS-NavigationModel*; otherwise it is not present. |
| *RTISup* | The field is mandatory present if the target device supports *GNSS-RealTimeIntegrity*; otherwise it is not present. |
| *DataBitsSup* | The field is mandatory present if the target device supports *GNSS-DataBitAssistance*; otherwise it is not present. |
| *AcquAssistSup* | The field is mandatory present if the target device supports *GNSS-AcquisitionAssistance*; otherwise it is not present. |
| *AlmanacSup* | The field is mandatory present if the target device supports *GNSS-Almanac*; otherwise it is not present. |
| *UTCModSup* | The field is mandatory present if the target device supports *GNSS-UTC-Model*; otherwise it is not present. |
| *AuxInfoSup* | The field is mandatory present if the target device supports *GNSS-AuxiliaryInformation*; otherwise it is not present. |
| *DBDS-Sup* | The field is mandatory present if the target device supports *BDS-DifferentialCorrections*; otherwise it is not present. This field may only be present if *gnss-ID* indicates 'bds'. |
| *BDS-GridModSup* | The field is mandatory present if the target device supports *BDS-GridModel*; otherwise it is not present. This field may only be present if *gnss-ID* indicates 'bds'. |
| *RTK-OSR-Sup* | The field is mandatory present if the target device supports *GNSS-RTK-Observations*; otherwise it is not present. Note, support for *GNSS-RTK-Observations* implies support for *GNSS-RTK-CommonObservationInfo* as well. |
| *GLO-CPB-Sup* | The field is mandatory present if the target device supports *GLO‑RTK‑BiasInformation*; otherwise it is not present. This field may only be present if *gnss-ID* indicates 'glonass'. |
| *MAC-Sup* | The field is mandatory present if the target device supports *GNSS‑RTK‑MAC‑CorrectionDifferences*; otherwise it is not present. |
| *Res-Sup* | The field is mandatory present if the target device supports *GNSS‑RTK‑Residuals*; otherwise it is not present. |
| *FKP-Sup* | The field is mandatory present if the target device supports *GNSS‑RTK‑FKP‑Gradients*; otherwise it is not present. |
| *OC-Sup* | The field is mandatory present if the target device supports *GNSS‑SSR‑OrbitCorrections*; otherwise it is not present. |
| *CC-Sup* | The field is mandatory present if the target device supports *GNSS‑SSR‑ClockCorrections*; otherwise it is not present. |
| *CB-Sup* | The field is mandatory present if the target device supports *GNSS‑SSR‑CodeBias*; otherwise it is not present. |
| *URA-Sup* | The field is mandatory present if the target device supports *GNSS-SSR-URA*; otherwise it is not present. |
| *PB-Sup* | The field is mandatory present if the target device supports *GNSS-SSR-PhaseBias*; otherwise it is not present. |
| *STEC-Sup* | The field is mandatory present if the target device supports *GNSS-SSR-STEC-Correction*; otherwise it is not present. |
| *Grid-Sup* | The field is mandatory present if the target device supports *GNSS‑SSR‑GriddedCorrection*; otherwise it is not present. Note, support for *GNSS‑SSR‑GriddedCorrection* implies support for *GNSS-SSR-CorrectionPoints* as well. |
| *DNavIC-Sup* | The field is mandatory present if the target device supports *NavIC-DifferentialCorrections*; otherwise it is not present. This field may only be present if the *gnss-ID* indicates 'navic'. |
| *NavIC-GridModSup* | The field is mandatory present if the target device supports *NavIC-GridModel*; otherwise it is not present. This field may only be present if the *gnss-ID* indicates 'navic'. |
| *OC2-Sup* | The field is mandatory present if the target device supports *GNSS‑SSR‑OrbitCorrectionsSet2*; otherwise it is not present. |
| *CC2-Sup* | The field is mandatory present if the target device supports *GNSS‑SSR‑ClockCorrectionsSet2*; otherwise it is not present. |
| *URA2-Sup* | The field is mandatory present if the target device supports *GNSS-SSR-URA-Set2*; otherwise it is not present. |
| *LOS-NLOS-Grid-Sup* | The field is mandatory present if the target device supports *GNSS-LOS-NLOS-GriddedIndications*; otherwise it is not present. Support for *GNSS-LOS-NLOS-GriddedIndications* implies support for *GNSS-LOS-NLOS-GridPoints*. |
| *SatPCV-Sup* | The field is mandatory present if the target device supports *GNSS-SSR-SatellitePCVResiduals*; otherwise it is not present. |

#### – *GNSS-TimeModelListSupport*

-- ASN1START

GNSS-TimeModelListSupport ::= SEQUENCE {

...

}

-- ASN1STOP

#### – *GNSS-DifferentialCorrectionSupport*

-- ASN1START

GNSS-DifferentialCorrectionsSupport ::= SEQUENCE {

gnssSignalIDs GNSS-SignalIDs,

dgnss-ValidityTimeSup BOOLEAN,

...

}

-- ASN1STOP

| *GNSS-DifferentialCorrectionsSupport* field descriptions |
| --- |
| ***gnssSignalIDs***  This field specifies the GNSS signal types for which differential corrections are supported by the target device. This is represented by a bit string in *GNSS-SignalIDs*, with a one‑value at the bit position means differential corrections for the particular GNSS signal type is supported; a zero‑value means not supported. |
| ***dgnss-ValidityTimeSup***  This field specifies if the target device supports estimation of UDRE based on growth rate and validity time for differential corrections. TRUE means supported. |

#### – *GNSS-NavigationModelSupport*

-- ASN1START

GNSS-NavigationModelSupport ::= SEQUENCE {

clockModel BIT STRING { model-1 (0),

model-2 (1),

model-3 (2),

model-4 (3),

model-5 (4),

model-6 (5),

model-7-r16 (6),

model-8-r16 (7) } (SIZE (1..8)) OPTIONAL,

orbitModel BIT STRING { model-1 (0),

model-2 (1),

model-3 (2),

model-4 (3),

model-5 (4),

model-6 (5),

model-7-r16 (6),

model-8-r16 (7) } (SIZE (1..8)) OPTIONAL,

...

}

-- ASN1STOP

| *GNSS-NavigationModelSupport* field descriptions |
| --- |
| ***clockModel***  This field specifies the *gnss-ClockModel* choice(s) in *GNSS-NavigationModel* IE supported by the target device for the GNSS indicated by *GNSS‑ID*. This is represented by a bit string, with a one‑value at the bit position means the particular clock model is supported; a zero‑value means not supported.  If the target device supports GPS and *GNSS-NavigationModel* assistance, it shall support *clockModel* Model-2.  If the target device supports SBAS and *GNSS-NavigationModel* assistance, it shall support *clockModel* Model-5.  If the target device supports QZSS and *GNSS-NavigationModel* assistance, it shall support *clockModel* Model-2.  If the target device supports Galileo and *GNSS-NavigationModel* assistance, it shall support *clockModel* Model-1.  If the target device supports GLONASS and *GNSS-NavigationModel* assistance, it shall support *clockModel* Model-4.  If the target device supports BDS and *GNSS-NavigationModel* assistance, it shall support *clockModel* Model-6.  If the target device supports NavIC and *GNSS-NavigationModel* assistance, it shall support *clockModel* Model-8.  If this field is absent, the target device supports the mandatory (native) *clockModel* choice only as listed above for the GNSS indicated by *GNSS‑ID*. |
| ***orbitModel***  This field specifies the *gnss-OrbitModel* choice(s) in *GNSS-NavigationModel* IE supported by the target device for the GNSS indicated by *GNSS‑ID*. This is represented by a bit string, with a one‑value at the bit position means the particular orbit model is supported; a zero‑value means not supported.  If the target device supports GPS and *GNSS-NavigationModel* assistance, it shall support *orbitModel* Model-2.  If the target device supports SBAS and *GNSS-NavigationModel* assistance, it shall support *orbitModel* Model-5.  If the target device supports QZSS and *GNSS-NavigationModel* assistance, it shall support *orbitModel* Model-2.  If the target device supports Galileo and *GNSS-NavigationModel* assistance, it shall support*orbitModel* Model-1.  If the target device supports GLONASS and *GNSS-NavigationModel* assistance, it shall support *orbitModel* Model-4.  If the target device supports BDS and *GNSS-NavigationModel* assistance, it shall support *orbitModel* Model-6.  If the target device supports NavIC and *GNSS-NavigationModel* assistance, it shall support *orbitModel* Model-8.  If this field is absent, the target device supports the mandatory (native) *orbitModel* choice only as listed above for the GNSS indicated by *GNSS‑ID*. |

#### – *GNSS-RealTimeIntegritySupport*

-- ASN1START

GNSS-RealTimeIntegritySupport ::= SEQUENCE {

...

}

-- ASN1STOP

#### – *GNSS-DataBitAssistanceSupport*

-- ASN1START

GNSS-DataBitAssistanceSupport ::= SEQUENCE {

...

}

-- ASN1STOP

#### – *GNSS-AcquisitionAssistanceSupport*

-- ASN1START

GNSS-AcquisitionAssistanceSupport ::= SEQUENCE {

...,

confidenceSupport-r10 ENUMERATED { true } OPTIONAL,

dopplerUncertaintyExtSupport-r10 ENUMERATED { true } OPTIONAL

}

-- ASN1STOP

| ***GNSS-AcquisitionAssistanceSupport* field descriptions** |
| --- |
| ***confidenceSupport***  If this field is present, the target device supports the *confidence* field in *GNSS-AcquisitionAssistance*. |
| ***dopplerUncertaintyExtSupport***  If this field is present, the target device supports the *dopplerUncertaintyExt* field in *GNSS-AcquisitionAssistance*. |

#### – *GNSS-AlmanacSupport*

-- ASN1START

GNSS-AlmanacSupport ::= SEQUENCE {

almanacModel BIT STRING { model-1 (0),

model-2 (1),

model-3 (2),

model-4 (3),

model-5 (4),

model-6 (5),

model-7 (6),

model-8-v16e0 (7) } (SIZE (1..8)) OPTIONAL,

...

}

-- ASN1STOP

| *GNSS-AlmanacSupport* field descriptions |
| --- |
| ***almanacModel***  This field specifies the *almanacModel* choice(s) in *GNSS-Almanac* IE supported by the target device for the GNSS indicated by *GNSS‑ID*. This is represented by a bit string, with a one‑value at the bit position means the particular almanac model is supported; a zero‑value means not supported.  If the target device supports GPS and *GNSS-Almanac* assistance, it shall support Model-2.  If the target device supports SBAS and *GNSS-Almanac* assistance, it shall support Model-6.  If the target device supports QZSS and *GNSS-Almanac* assistance, it shall support Model-2.  If the target device supports Galileo and *GNSS-Almanac* assistance, it shall support Model-1.  If the target device supports GLONASS and *GNSS-Almanac* assistance, it shall support Model-5.  If the target device supports BDS and *GNSS-Almanac* assistance, it shall support Model-7.  If the target device supports NavIC and *GNSS-Almanac* assistance, it shall support Model-8.  If this field is absent, the target device supports the mandatory (native) *almanacModel* choice only as listed above for the GNSS indicated by *GNSS‑ID*. |

#### – *GNSS-UTC-ModelSupport*

-- ASN1START

GNSS-UTC-ModelSupport ::= SEQUENCE {

utc-Model BIT STRING { model-1 (0),

model-2 (1),

model-3 (2),

model-4 (3),

model-5 (4) } (SIZE (1..8)) OPTIONAL,

...

}

-- ASN1STOP

| *GNSS-UTC-ModelSupport* field descriptions |
| --- |
| ***utc-Model***  This field specifies the *GNSS-UTC-Model* choice(s) in *GNSS-UTC-Model* IE supported by the target device for the GNSS indicated by *GNSS‑ID*. This is represented by a bit string, with a one‑value at the bit position means the particular UTC model is supported; a zero‑value means not supported.  If the target device supports GPS and *GNSS-UTC-Model* assistance, it shall support Model-1.  If the target device supports SBAS and *GNSS-UTC-Model* assistance, it shall support Model-4.  If the target device supports QZSS and *GNSS-UTC-Model* assistance, it shall support Model-1.  If the target device supports Galileo and *GNSS-UTC-Model* assistance, it shall support Model-1.  If the target device supports GLONASS and *GNSS-UTC-Model* assistance, it shall support Model-3.  If the target device supports BDS and *GNSS-UTC-Model* assistance, it shall support Model-5.  If the target device supports NavIC and *GNSS-UTC-Model* assistance, it shall support Model-2.  If this field is absent, the target device supports the mandatory (native) *utc-Model* choice only as listed above for the GNSS indicated by *GNSS‑ID*. |

#### – *GNSS-AuxiliaryInformationSupport*

-- ASN1START

GNSS-AuxiliaryInformationSupport ::= SEQUENCE {

...

}

-- ASN1STOP

#### – *BDS-DifferentialCorrectionsSupport*

-- ASN1START

BDS-DifferentialCorrectionsSupport-r12 ::= SEQUENCE {

gnssSignalIDs GNSS-SignalIDs,

...

}

-- ASN1STOP

| *BDS-DifferentialCorrectionsSupport* field descriptions |
| --- |
| ***gnssSignalIDs***  This field specifies the BDS signal types for which differential corrections are supported by the target device. This is represented by a bit string in *GNSS-SignalIDs*, with a one‑value at the bit position means differential corrections for the particular BDS signal type is supported; a zero‑value means not supported. |

#### – *BDS-GridModelSupport*

-- ASN1START

BDS-GridModelSupport-r12 ::= SEQUENCE {

...

}

-- ASN1STOP

#### – *GNSS-RTK-ObservationsSupport*

-- ASN1START

GNSS-RTK-ObservationsSupport-r15 ::= SEQUENCE {

gnssSignalIDs-r15 GNSS-SignalIDs,

...

}

-- ASN1STOP

| *GNSS-RTK-ObservationsSupport* field descriptions |
| --- |
| ***gnssSignalIDs***  This field specifies the GNSS signal types for which *GNSS-RTK-Observations* are supported by the target device. This is represented by a bit string in *GNSS-SignalIDs*, with a one‑value at the bit position means *GNSS‑RTK‑Observations* for the particular GNSS signal type is supported; a zero‑value means not supported. |

#### – *GLO-RTK-BiasInformationSupport*

-- ASN1START

GLO-RTK-BiasInformationSupport-r15 ::= SEQUENCE {

...

}

-- ASN1STOP

#### – *GNSS-RTK-MAC-CorrectionDifferencesSupport*

-- ASN1START

GNSS-RTK-MAC-CorrectionDifferencesSupport-r15 ::= SEQUENCE {

link-combinations-support-r15 GNSS-Link-CombinationsList-r15,

...

}

-- ASN1STOP

| *GNSS-RTK-MAC-CorrectionDifferencesSupport* field descriptions |
| --- |
| ***link-combinations-support***  This field specifies the GNSS link/frequency combinations for which *GNSS-RTK-MAC-CorrectionDifferences* are supported by the target device for the GNSS indicated by *GNSS-ID*. |

#### – *GNSS-RTK-ResidualsSupport*

-- ASN1START

GNSS-RTK-ResidualsSupport-r15 ::= SEQUENCE {

link-combinations-support-r15 GNSS-Link-CombinationsList-r15,

...

}

-- ASN1STOP

| *GNSS-RTK-ResidualsSupport* field descriptions |
| --- |
| ***link-combinations-support***  This field specifies the GNSS link/frequency combinations for which *GNSS-RTK-Residuals* are supported by the target device for the GNSS indicated by *GNSS-ID*. |

#### – *GNSS-RTK-FKP-GradientsSupport*

-- ASN1START

GNSS-RTK-FKP-GradientsSupport-r15 ::= SEQUENCE {

link-combinations-support-r15 GNSS-Link-CombinationsList-r15,

...

}

-- ASN1STOP

| *GNSS-RTK-FKP-GradientsSupport* field descriptions |
| --- |
| ***link-combinations-support***  This field specifies the GNSS link/frequency combinations for which *GNSS-RTK-FKP-Gradients* are supported by the target device for the GNSS indicated by *GNSS-ID*. |

#### – *GNSS-SSR-OrbitCorrectionsSupport*

-- ASN1START

GNSS-SSR-OrbitCorrectionsSupport-r15 ::= SEQUENCE {

...,

[[

orbit-IntegritySup-r17 BIT STRING { correlationTimeSup (0)

} (SIZE(1..8)) OPTIONAL

]]

}

-- ASN1STOP

| *GNSS-SSR-OrbitCorrectionsSupport* field descriptions |
| --- |
| ***orbit-IntegritySup***  This field, if present, indicates that the target device supports the IEs *ORBIT-IntegrityParameters* and *SSR-IntegrityOrbitBounds*.  A one‑value at the bit position '0' means that the target device supports the fields *orbitRangeErrorCorrelationTime* and *orbitRangeRateErrorCorrelationTime* in IE *ORBIT-IntegrityParameters*. |

#### – *GNSS-SSR-ClockCorrectionsSupport*

-- ASN1START

GNSS-SSR-ClockCorrectionsSupport-r15 ::= SEQUENCE {

...,

[[

clock-IntegrityParameterSupport-r17 ENUMERATED { supported } OPTIONAL,

ssr-IntegrityClockBoundsSupport-r17 ENUMERATED { supported } OPTIONAL

]]

}

-- ASN1STOP

| *GNSS-SSR-ClockCorrectionsSupport* field descriptions |
| --- |
| ***clock-IntegrityParameterSupport***  This field, if present, indicates that the target device supports the *CLOCK-IntegrityParameters* in IE *GNSS-SSR-ClockCorrections*. |
| ***ssr-IntegrityClockBoundsSupports***  This field. If present, indicates that the target device supports the *SSR-IntegrityClockBounds* in IE *GNSS-SSR-ClockCorrections*. |

– *GNSS-SSR-CodeBiasSupport*

-- ASN1START

GNSS-SSR-CodeBiasSupport-r15 ::= SEQUENCE {

signal-and-tracking-mode-ID-Sup-r15 GNSS-SignalIDs,

...,

[[

ssr-IntegrityCodeBiasBoundsSup-r17 ENUMERATED { supported } OPTIONAL

]]

}

-- ASN1STOP

| GNSS-SSR-CodeBiasSupport field descriptions |
| --- |
| ***signal-and-tracking-mode-ID-Sup***  This field specifies the GNSS signal(s) for which the *GNSS-SSR-CodeBias* is supported by the target device. |
| ***ssr-IntegrityCodeBiasBoundsSup***  This field, if present, indicates that the target device supports the IE *SSR-IntegrityCodeBiasBounds*. |

#### – *GNSS-SSR-URA-Support*

-- ASN1START

GNSS-SSR-URA-Support-r16 ::= SEQUENCE {

...

}

-- ASN1STOP

– *GNSS-SSR-PhaseBiasSupport*

-- ASN1START

GNSS-SSR-PhaseBiasSupport-r16 ::= SEQUENCE {

signal-and-tracking-mode-ID-Sup-r16 GNSS-SignalIDs,

...,

[[

ssr-IntegrityPhaseBiasBoundsSup-r17 ENUMERATED { supported } OPTIONAL

]]

}

-- ASN1STOP

| *GNSS-SSR-PhaseBiasSupport* field descriptions |
| --- |
| ***signal-and-tracking-mode-ID-Sup***  This field specifies the GNSS signal(s) for which the *GNSS-SSR-PhaseBias* is supported by the target device. |
| ***ssr-IntegrityPhaseBiasBoundsSup***  This field, if present, indicates that the target device supports the IE *SSR-IntegrityPhaseBiasBounds*. |

#### – *GNSS-SSR-STEC-CorrectionSupport*

-- ASN1START

GNSS-SSR-STEC-CorrectionSupport-r16 ::= SEQUENCE {

...,

[[

stec-IntegritySup-r17 BIT STRING { correlationTimeSup (0)

} (SIZE(1..8)) OPTIONAL

]]

}

-- ASN1STOP

| *GNSS-SSR-STEC-CorrectionSupport* field descriptions |
| --- |
| ***stec-IntegritySup***  This field, if present, indicates that the target device supports the IEs *STEC-IntegrityParameters* and *STEC-IntegrityErrorBounds*.  A one‑value at the bit position '0' means that the target device supports the fields *ionoRangeErrorCorrelationTime* and *ionoRangeRateErrorCorrelationTime* in IE *STEC-IntegrityParameters*. |

#### – *GNSS-SSR-GriddedCorrectionSupport*

-- ASN1START

GNSS-SSR-GriddedCorrectionSupport-r16 ::= SEQUENCE {

...,

[[

griddedCorrectionIntegritySup-r17 ENUMERATED { supported } OPTIONAL

]]

}

-- ASN1STOP

| *GNSS-SSR-GriddedCorrectionSupport* field descriptions |
| --- |
| ***griddedCorrectionIntegritySup***  This field, if present, indicates that the target device supports the IEs *SSR-GriddedCorrectionIntegrityParameters* and *TropoDelayIntegrityErrorBounds*. |

#### – *NavIC-DifferentialCorrectionsSupport*

-- ASN1START

NavIC-DifferentialCorrectionsSupport-r16 ::= SEQUENCE {

gnssSignalIDs-r16 GNSS-SignalIDs,

...

}

-- ASN1STOP

| *NavIC-DifferentialCorrectionsSupport* field descriptions |
| --- |
| ***gnssSignalIDs***  This field specifies the NavIC signal types for which differential corrections are supported by the target device. This is represented by a bit string in *GNSS-SignalIDs*, with a one‑value at the bit position means differential corrections for the particular NavIC signal type is supported; a zero‑value means not supported. |

#### – *NavIC-GridModelSupport*

-- ASN1START

NavIC-GridModelSupport-r16 ::= SEQUENCE {

...

}

-- ASN1STOP

#### – *GNSS-SSR-OrbitCorrectionsSet2Support*

-- ASN1START

GNSS-SSR-OrbitCorrectionsSet2Support-r17 ::= SEQUENCE {

...

}

-- ASN1STOP

#### – *GNSS-SSR-ClockCorrectionsSet2Support*

-- ASN1START

GNSS-SSR-ClockCorrectionsSet2Support-r17 ::= SEQUENCE {

...

}

-- ASN1STOP

#### – *GNSS-SSR-URA-Set2Support*

-- ASN1START

GNSS-SSR-URA-Set2Support-r17 ::= SEQUENCE {

...

}

-- ASN1STOP

#### – *GNSS-LOS-NLOS-GriddedIndicationsSupport*

-- ASN1START

GNSS-LOS-NLOS-GriddedIndicationsSupport-r18 ::= SEQUENCE {

...

}

-- ASN1STOP

– *GNSS-SSR-SatellitePCVResidualsSupport*

-- ASN1START

GNSS-SSR-SatellitePCVResidualsSupport-r18 ::= SEQUENCE {

...

}

-- ASN1STOP

#### 6.5.2.11 GNSS Capability Information Request

#### – *A-GNSS-RequestCapabilities*

The IE *A-GNSS-Request-Capabilities* is used by the location server to request A-GNSS location capabilities (e.g., GNSSs and assistance data supported) from the target device.

-- ASN1START

A-GNSS-RequestCapabilities ::= SEQUENCE {

gnss-SupportListReq BOOLEAN,

assistanceDataSupportListReq BOOLEAN,

locationVelocityTypesReq BOOLEAN,

...

}

-- ASN1STOP

| *A-GNSS-RequestCapabilities* field descriptions |
| --- |
| ***gnss-SupportListReq***  This field specifies whether the target device is requested to include the *gnss-SupportList* field in the *A-GNSS-ProvideCapabilities* IE or not. TRUE means requested. |
| ***assistanceDataSupportListReq***  This field specifies whether the target device is requested to include the *assistanceDataSupportList* field in the *A‑GNSS‑ProvideCapabilities* IE or not. TRUE means requested. |
| ***locationVelocityTypesReq***  This field specifies whether the target device is requested to include the *locationCoordinateTypes* field and *velocityTypes* field in the *A-GNSS-ProvideCapabilities* IE or not. TRUE means requested. |

#### 6.5.2.12 GNSS Error Elements

#### – *A-GNSS-Error*

The IE *A-GNSS-Error* is used by the location server or target device to provide GNSS error reasons.

-- ASN1START

A-GNSS-Error ::= CHOICE {

locationServerErrorCauses GNSS-LocationServerErrorCauses,

targetDeviceErrorCauses GNSS-TargetDeviceErrorCauses,

...

}

-- ASN1STOP

#### – *GNSS-LocationServerErrorCauses*

The IE *GNSS-LocationServerErrorCauses* is used by the location server to provide GNSS error reasons to the target device.

-- ASN1START

GNSS-LocationServerErrorCauses ::= SEQUENCE {

cause ENUMERATED {

undefined,

undeliveredAssistanceDataIsNotSupportedByServer,

undeliveredAssistanceDataIsSupportedButCurrentlyNotAvailableByServer, undeliveredAssistanceDataIsPartlyNotSupportedAndPartlyNotAvailableByServer,

...,

unconfirmedPeriodicAssistanceDataIsNotSupported-v1510,

unconfirmedPeriodicAssistanceDataIsSupportedButCurrentlyNotAvailable-v1510,

unconfirmedPeriodicAssistanceDataIsPartlyNotSupportedAndPartlyNotAvailable-v1510,

undeliveredPeriodicAssistanceDataIsCurrentlyNotAvailable-v1510

},

...

}

-- ASN1STOP

| *GNSS-LocationServerErrorCauses* field descriptions |
| --- |
| ***cause***  This field provides a GNSS specific error cause. The cause values '*unconfirmedPeriodicAssistanceDataIsNotSupported'*, '*unconfirmedPeriodicAssistanceDataIsSupportedButCurrentlyNotAvailable*' and '*unconfirmedPeriodicAssistanceDataIsPartlyNotSupportedAndPartlyNotAvailable*' may only be included in the control transaction of a periodic assistance data transfer procedure, as described in clause 5.2.1a.  The cause value '*undeliveredPeriodicAssistanceDataIsCurrentlyNotAvailable*' may only be included in the data transaction of a periodic assistance data transfer procedure when periodic assistance data are not available when the periodicity condition occurs, as described in clauses 5.2.1a and 5.2.2a. |

#### – *GNSS-TargetDeviceErrorCauses*

The IE *GNSS-TargetDeviceErrorCauses* is used by the target device to provide GNSS error reasons to the location server.

-- ASN1START

GNSS-TargetDeviceErrorCauses ::= SEQUENCE {

cause ENUMERATED { undefined,

thereWereNotEnoughSatellitesReceived,

assistanceDataMissing,

notAllRequestedMeasurementsPossible,

...

},

fineTimeAssistanceMeasurementsNotPossible NULL OPTIONAL,

adrMeasurementsNotPossible NULL OPTIONAL,

multiFrequencyMeasurementsNotPossible NULL OPTIONAL,

...,

[[

remoteUE-Indication-r18 ENUMERATED {true} OPTIONAL -- Cond NR

]]

}

-- ASN1STOP

| Conditional presence | Explanation |
| --- | --- |
| *NR* | This field is optionally present, need OR, for NR access. Otherwise it is not present. |

| *GNSS-TargetDeviceErrorCauses* field descriptions |
| --- |
| ***cause***  This field provides a GNSS specific error cause. If the cause value is '*notAllRequestedMeasurementsPossible*', the target device was not able to provide all requested GNSS measurements (but may be able to report a location estimate or location measurements). In this case, the target device should include any of the *fineTimeAssistanceMeasurementsNotPossible*, *adrMeasurementsNotPossible*, or *multiFrequenceMeasurementsNotPossible* fields, as applicable. |
| ***remoteUE-Indication***  This field indicates whether the target device in NR access is configured as a L2 U2N Remote UE. |

#### 6.5.2.13 Common GNSS Information Elements

#### – *GNSS-FrequencyID*

The IE *GNSS-FrequencyID* is used to indicate a specific GNSS link/frequency. The interpretation of *GNSS‑FrequencyID* depends on the *GNSS‑ID.*

-- ASN1START

GNSS-FrequencyID-r15 ::= SEQUENCE {

gnss-FrequencyID-r15 INTEGER (0 .. 7),

...

}

-- ASN1STOP

| *GNSS-FrequencyID* field descriptions |
| --- |
| ***gnss-FrequencyID***  This field specifies a particular GNSS link/frequency. The interpretation of *gnss-FrequencyID* depends on the *GNSS‑ID* and is as shown in the table Value & Explanation relation below. |

Value & Explanation relation

|  |  |  |  |
| --- | --- | --- | --- |
| System | Value | Explanation | |
| Link | Centre Frequency  [MHz] |
| GPS | 0 | L1 | 1575.42 |
| 1 | L2 | 1227.60 |
| 2 | L5 | 1176.45 |
| 3-7 | reserved | |
| SBAS | 0 | L1 | 1575.42 |
| 1 | L5 | 1176.45 |
| 2-7 | reserved | |
| QZSS | 0 | L1 | 1575.42 |
| 1 | L2 | 1227.60 |
| 2 | L5 | 1176.45 |
| 3-7 | reserved | |
| GLONASS  k = -7..13 | 0 | G1 | 1602+k×0.5625 |
| 1 | G2 | 1246+k×0.4375 |
| 2 | G3 | 1202.025 |
| 3-7 | reserved | |
| Galileo | 0 | E1 | 1575.420 |
| 1 | E6 | 1278.750 |
| 2 | E5a | 1176.450 |
| 3 | E5b | 1207.140 |
| 4 | E5 | 1191.795 |
|  | 5-7 | reserved | |
| BDS | 0 | B1I | 1561.098 |
| 1 | B1C | 1575.420 |
| 2 | B2 | 1207.140 |
|  | 3 | B3 | 1268.520 |
|  | 4 | B2a | 1176.450 |
|  | 5-7 | reserved | |
| NavIC | 0 | L5 | 1176.450 |
|  | 1-7 | reserved | |

#### – *GNSS-ID*

The IE *GNSS-ID* is used to indicate a specific GNSS.

-- ASN1START

GNSS-ID ::= SEQUENCE {

gnss-id ENUMERATED{ gps, sbas, qzss, galileo, glonass, ..., bds, navic-v1610 },

...

}

-- ASN1STOP

#### – *GNSS-ID-Bitmap*

The IE *GNSS-ID-Bitmap* is used to indicate several GNSSs using a bit map.

-- ASN1START

GNSS-ID-Bitmap ::= SEQUENCE {

gnss-ids BIT STRING { gps (0),

sbas (1),

qzss (2),

galileo (3),

glonass (4),

bds (5),

navic-v1610 (6) } (SIZE (1..16)),

...

}

-- ASN1STOP

| *GNSS-ID-Bitmap* field descriptions |
| --- |
| ***gnss‑ids***  This field specifies the GNSS(s). This is represented by a bit string, with a one‑value at the bit position means the particular GNSS is addressed; a zero‑value means not addressed. |

#### – *GNSS-Link-CombinationsList*

-- ASN1START

GNSS-Link-CombinationsList-r15 ::= SEQUENCE (SIZE(1..8)) OF GNSS-Link-Combinations-r15

GNSS-Link-Combinations-r15 ::= SEQUENCE {

l1-r15 GNSS-FrequencyID-r15,

l2-r15 GNSS-FrequencyID-r15,

...

}

-- ASN1STOP

#### – *GNSS-NavListInfo*

-- ASN1START

GNSS-NavListInfo-r15 ::= SEQUENCE (SIZE (1..64)) OF SatListElement-r15

SatListElement-r15 ::= SEQUENCE {

svID-r15 SV-ID,

iod-r15 BIT STRING (SIZE(11)),

...

}

-- ASN1STOP

#### – *GNSS-NetworkID*

The IE *GNSS-NetworkID* defines the reference network and the source of the particular set of reference stations and their observation information. This IE is used for MAC Network RTK as described in [30].

-- ASN1START

GNSS-NetworkID-r15 ::= SEQUENCE {

networkID-r15 INTEGER (0..255),

...

}

-- ASN1STOP

#### – *GNSS-PeriodicControlParam*

The IE *GNSS-PeriodicControlParam* is used to specify control parameters for a periodic assistance data delivery.

-- ASN1START

GNSS-PeriodicControlParam-r15 ::= SEQUENCE {

deliveryAmount-r15 INTEGER (1..32),

deliveryInterval-r15 INTEGER (1..64),

...

}

-- ASN1STOP

| *GNSS-PeriodicControlParam* field descriptions |
| --- |
| ***deliveryAmount***  This field specifies the number of periodic assistance data deliveries. Integer values *N*=1…31 correspond to an amount of 2*N*. Integer value *N*=32 indicates an 'infinite/indefinite' amount, which means that the assistance data delivery should continue until a LPP *Abort* message is received. |
| ***deliveryInterval***  This field specifies the interval between assistance data deliveries in seconds. |

#### – *GNSS-ReferenceStationID*

The IE *GNSS-ReferenceStationID* is used to identify a specific GNSS Reference Station.

-- ASN1START

GNSS-ReferenceStationID-r15 ::= SEQUENCE {

referenceStationID-r15 INTEGER (0..65535),

providerName-r15 VisibleString (SIZE (1..32)) OPTIONAL, -- Need ON

...

}

-- ASN1STOP

| *GNSS-ReferenceStationID* field descriptions |
| --- |
| ***referenceStationID***  This field provides the reference station identity. |
| ***providerName***  This field is associated with a GNSS correction data provider to ensure that the *referenceStationID*'s are unique from a target device perspective. |

#### – *GNSS-SignalID*

The IE *GNSS-SignalID* is used to indicate a specific GNSS signal type. The interpretation of *GNSS-SignalID* depends on the *GNSS‑ID.*

-- ASN1START

GNSS-SignalID ::= SEQUENCE {

gnss-SignalID INTEGER (0 .. 7),

...,

[[

gnss-SignalID-Ext-r15 INTEGER (8..23) OPTIONAL -- Need ON

]]

}

-- ASN1STOP

| *GNSS-SignalID* field descriptions |
| --- |
| ***gnss-SignalID, gnss-SignalID-Ext***  This field specifies a particular GNSS signal. The interpretation of *gnss-SignalID* and *gnss-SignalID-Ext* depends on the *GNSS‑ID* and is as shown in the table System to Value & Explanation relation below.  If the field *gnss-SignalID-Ext* is present, the *gnss-SignalID* should be set to value 7 and shall be ignored by the receiver. |

System to Value & Explanation relation

|  |  |  |
| --- | --- | --- |
| System | Value | Explanation |
| GPS | 0 | GPS L1 C/A |
| 1 | GPS L1C |
| 2 | GPS L2C |
| 3 | GPS L5 |
| 4 | GPS L1 P |
| 5 | GPS L1 Z-tracking |
| 6 | GPS L2 C/A |
| 7 | GPS L2 P |
| 8 | GPS L2 Z-tracking |
| 9 | GPS L2 L2C(M) |
| 10 | GPS L2 L2C(L) |
| 11 | GPS L2 L2C(M+L) |
| 12 | GPS L5 I |
| 13 | GPS L5 Q |
| 14 | GPS L5 I+Q |
| 15 | GPS L1 L1C(D) |
| 16 | GPS L1 L1C(P) |
| 17 | GPS L1 L1C(D+P) |
| 18-23 | Reserved |
| SBAS | 0 | L1 C/A |
| 1 | L5 I |
| 2 | L5 Q |
| 3 | L5 I+Q |
| 4-7 | Reserved |
| QZSS | 0 | QZS-L1 C/A |
| 1 | QZS-L1C |
| 2 | QZS-L2C |
| 3 | QZS-L5 |
| 4 | QZS-LEX S |
| 5 | QZS-LEX L |
| 6 | QZS-LEX S+L |
| 7 | QZS-L2 L2C(M) |
| 8 | QZS-L2 L2C(L) |
| 9 | QZS-L2 L2C(M+L) |
| 10 | QZS-L5 I |
| 11 | QZS-L5 Q |
| 12 | QZS-L5 I+Q |
| 13 | QZS L1 L1C(D) |
| 14 | QZS L1 L1C(P) |
| 15 | QZS L1 L1C(D+P) |
| 16-23 | Reserved |
| GLONASS | 0 | GLONASS G1 C/A |
| 1 | GLONASS G2 C/A |
| 2 | GLONASS G3 |
| 3 | GLONASS G1 P |
| 4 | GLONASS G2 P |
| 5 | GLONASS G1a(D) |
| 6 | GLONASS G1a(P) |
| 7 | GLONASS G1a (D+P) |
| 8 | GLONASS G2a(I) |
| 9 | GLONASS G2a(P) |
| 10 | GLONASS G2a(I+P) |
| 11 | GLONASS G3 I |
| 12 | GLONASS G3 Q |
| 13 | GLONASS G3 I+Q |
| 14-23 | Reserved |
| Galileo | 0 | Galileo E1 |
| 1 | Galileo E5A |
| 2 | Galileo E5B |
| 3 | Galileo E6 |
| 4 | Galileo E5A + E5B |
| 5 | Galileo E1 C No data |
| 6 | Galileo E1 A |
| 7 | Galileo E1 B I/NAV OS/CS/SoL |
| 8 | Galileo E1 B+C |
| 9 | Galileo E1 A+B+C |
| 10 | Galileo E6 C |
| 11 | Galileo E6 A |
| 12 | Galileo E6 B |
| 13 | Galileo E6 B+C |
| 14 | Galileo E6 A+B+C |
| 15 | Galileo E5B I |
| 16 | Galileo E5B Q |
| 17 | Galileo E5B I+Q |
| 18 | Galileo E5(A+B) I |
| 19 | Galileo E5(A+B) Q |
| 20 | Galileo E5(A+B) I+Q |
| 21 | Galileo E5A I |
| 22 | Galileo E5A Q |
| 23 | Galileo E5A I+Q |
| BDS | 0 | B1 I |
| 1 | B1 Q |
| 2 | B1 I+Q |
| 3 | B3 I |
| 4 | B3 Q |
| 5 | B3 I+Q |
| 6 | B2 I |
| 7 | B2 Q |
| 8 | B2 I+Q |
| 9 | B1C(D) |
| 10 | B1C(P) |
| 11 | B1C(D+P) |
| 12 | B2a(D) |
| 13 | B2a(P) |
| 14 | B2a(D+P) |
| 15-23 | Reserved |
| NavIC | 0 | NavIC L5 SPS |
| 1-23 | Reserved |

#### – *GNSS-SignalIDs*

The IE *GNSSSignal‑IDs* is used to indicate several GNSS signals using a bit map. The interpretation of *GNSSSignal‑IDs* depends on the *GNSS‑ID.*

-- ASN1START

GNSS-SignalIDs ::= SEQUENCE {

gnss-SignalIDs BIT STRING (SIZE(8)),

...,

[[

gnss-SignalIDs-Ext-r15 BIT STRING (SIZE(16)) OPTIONAL -- Need ON

]]

}

-- ASN1STOP

| *GNSS-SignalIDs* field descriptions |
| --- |
| ***gnss-SignalIDs, gnss-SignalIDs-Ext***  This field specifies one or several GNSS signals using a bit map. A one‑value at the bit position means the particular signal is addressed; a zero‑value at the particular bit position means the signal is not addressed. The interpretation of the bit map in *gnssSignalIDs* and *gnss-SignalIDs-Ext* depends on the *GNSS‑ID* and is shown in the table below.  Unfilled table entries indicate no assignment and shall be set to zero. |

Interpretation of the bit map in *gnssSignalIDs*

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| GNSS | Bit 1  (MSB) | Bit 2 | Bit 3 | Bit 4 | Bit 5 | Bit 6 | Bit 7 | Bit 8  (LSB) |
| GPS | L1 C/A | L1C | L2C | L5 | L1P | L1 Z | L2 C/A | L2 P |
| SBAS | L1 C/A | L5 I | L5 Q | L5 I+Q |  |  |  |  |
| QZSS | QZS-L1 C/A | QZS-L1C | QZS-L2C | QZS-L5 | LEX S | LEX L | LEX S+L | L2C(M) |
| GLONASS | G1 C/A | G2 C/A | G3 | G1 P | G2 P | G1a(D) | G1a(P) | G1a(D+P) |
| Galileo | E1 | E5a | E5b | E6 | E5a+E5b | E1 C No Data | E1 A | E1 B I/NAV OS/CS/SoL |
| BDS | B1 I | B1 Q | B1 I+Q | B3 I | B3 Q | B3 I+Q | B2 I | B2 Q |
| NavIC | L5 SPS |  |  |  |  |  |  |  |

Interpretation of the bit map in *gnssSignalIDs-Ext*

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| GNSS | Bit 1  (MSB) | Bit 2 | Bit 3 | Bit 4 | Bit 5 | Bit 6 | Bit 7 | Bit 8 |
| GPS | L2 Z | L2C(M) | L2C(L) | L2C(M+L) | L5 I | L5 Q | L5 I+Q | L1C(D) |
| SBAS |  |  |  |  |  |  |  |  |
| QZSS | L2C(L) | L2C(M+L) | L5 I | L5 Q | L5 I+Q | L1C(D) | L1C(P) | L1C(D+P) |
| GLONASS | G2a(I) | G2a(P) | G2a(I+P) | G3 I | G3 Q | G3(I+Q) |  |  |
| Galileo | E1 B+C | E1 A+B+C | E6C | E6A | E6B | E6 B+C | E6 A+B+C | E5B I |
| BDS | B2 I+Q | B1C(D) | B1C(P) | B1C(D+P) | B2a(D) | B2a(P) | B2a(D+P) |  |
| NavIC |  |  |  |  |  |  |  |  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| GNSS | Bit 9 | Bit 10 | Bit 11 | Bit 12 | Bit 13 | Bit 14 | Bit 15 | Bit 16  (LSB) |
| GPS | L1C(P) | L1C(D+P) |  |  |  |  |  |  |
| SBAS |  |  |  |  |  |  |  |  |
| QZSS |  |  |  |  |  |  |  |  |
| GLONASS |  |  |  |  |  |  |  |  |
| Galileo | E5B Q | E5B I+Q | E5(A+B) I | E5(A+B) Q | E5(A+B) I+Q | E5A I | E5A Q | E5A I+Q |
| BDS |  |  |  |  |  |  |  |  |
| NavIC |  |  |  |  |  |  |  |  |

#### – *GNSS-SubNetworkID*

The IE *GNSS-SubNetworkID* defines the subnetwork of a network identified by *GNSS-NetworkID*. This IE is used for MAC Network RTK as described in [30].

-- ASN1START

GNSS-SubNetworkID-r15 ::= SEQUENCE {

subNetworkID-r15 INTEGER (0..15),

...

}

-- ASN1STOP

#### – *SBAS-ID*

The IE *SBAS‑ID* is used to indicate a specific SBAS.

-- ASN1START

SBAS-ID ::= SEQUENCE {

sbas-id ENUMERATED { waas, egnos, msas, gagan, ...},

...

}

-- ASN1STOP

#### – *SBAS-IDs*

The IE *SBAS‑IDs* is used to indicate several SBASs using a bit map.

-- ASN1START

SBAS-IDs ::= SEQUENCE {

sbas-IDs BIT STRING { waas (0),

egnos (1),

msas (2),

gagan (3) } (SIZE (1..8)),

...

}

-- ASN1STOP

| *SBAS‑IDs* field descriptions |
| --- |
| ***sbas-IDs***  This field specifies one or several SBAS(s) using a bit map. A one‑value at the bit position means the particular SBAS is addressed; a zero‑value at the particular bit position means the SBAS is not addressed. |

#### – *SV-ID*

The IE *SV‑ID* is used to indicate a specific GNSS satellite. The interpretation of *SV‑ID* depends on the *GNSS‑ID.*

-- ASN1START

SV-ID ::= SEQUENCE {

satellite-id INTEGER(0..63),

...

}

-- ASN1STOP

| *SV‑ID* field descriptions |
| --- |
| ***satellite‑id***  This field specifies a particular satellite within a specific GNSS. The interpretation of *satellite‑id* depends on the *GNSS‑ID* see the table below. |

Interpretation of *satellite‑id*

|  |  |  |
| --- | --- | --- |
| System | Value of *satellite‑id* | Interpretation of *satellite‑id* |
| GPS | '0' – '62'  '63' | Satellite PRN Signal No. 1 to 63  Reserved |
| SBAS | '0' – '38'  '39' – '63' | Satellite PRN Signal No. 120 to 158  Reserved |
| QZSS | '0' – '9'  '10' – '63' | Satellite PRN Signal No. 193 to 202  Reserved |
| GLONASS | '0' – '23'  '24 – '63' | Slot Number 1 to 24  Reserved |
| Galileo | '0' – '35' '36' – '63' | Code No. 1 to 36 Reserved |
| BDS | '0' – '62'  '63' | Satellite ranging code number No.1 to 63  Reserved |
| NavIC | '0' – '13'  '14'–'63' | Satellite PRN Signal No. 1 to 14 Reserved |

### 6.5.3 Enhanced Cell ID Positioning

#### 6.5.3.1 E‑CID Location Information

#### – *ECID-ProvideLocationInformation*

The IE *ECID-ProvideLocationInformation* is used by the target device to provide E‑CID location measurements to the location server. It may also be used to provide E-CID positioning specific error reason.

-- ASN1START

ECID-ProvideLocationInformation ::= SEQUENCE {

ecid-SignalMeasurementInformation ECID-SignalMeasurementInformation OPTIONAL,

ecid-Error ECID-Error OPTIONAL,

...

}

-- ASN1STOP

#### 6.5.3.2 E‑CID Location Information Elements

#### – *ECID-SignalMeasurementInformation*

The IE *ECID-SignalMeasurementInformation* is used by the target device to provide various UE‑measurements to the location server.

-- ASN1START

ECID-SignalMeasurementInformation ::= SEQUENCE {

primaryCellMeasuredResults MeasuredResultsElement OPTIONAL,

measuredResultsList MeasuredResultsList,

...

}

MeasuredResultsList ::= SEQUENCE (SIZE(1..32)) OF MeasuredResultsElement

MeasuredResultsElement ::= SEQUENCE {

physCellId INTEGER (0..503),

cellGlobalId CellGlobalIdEUTRA-AndUTRA OPTIONAL,

arfcnEUTRA ARFCN-ValueEUTRA,

systemFrameNumber BIT STRING (SIZE (10)) OPTIONAL,

rsrp-Result INTEGER (0..97) OPTIONAL,

rsrq-Result INTEGER (0..34) OPTIONAL,

ue-RxTxTimeDiff INTEGER (0..4095) OPTIONAL,

...,

[[ arfcnEUTRA-v9a0 ARFCN-ValueEUTRA-v9a0 OPTIONAL -- Cond EARFCN-max

]],

[[ nrsrp-Result-r14 INTEGER (0..113) OPTIONAL,

nrsrq-Result-r14 INTEGER (0..74) OPTIONAL,

carrierFreqOffsetNB-r14 CarrierFreqOffsetNB-r14 OPTIONAL, -- Cond NB-IoT

hyperSFN-r14 BIT STRING (SIZE (10)) OPTIONAL

]],

[[

rsrp-Result-v1470 INTEGER (-17..-1) OPTIONAL,

rsrq-Result-v1470 INTEGER (-30..46) OPTIONAL

]]

}

-- ASN1STOP

|  |  |
| --- | --- |
| Conditional presence | Explanation |
| *EARFCN-max* | The field is mandatory present if the corresponding *arfcnEUTRA* (i.e. without suffix) is set to *maxEARFCN*. Otherwise the field is not present. |
| *NB-IoT* | The field is mandatory present if the measured cell is a NB-IoT cell. Otherwise it is not present. |

| *ECID-SignalMeasurementInformation* field descriptions |
| --- |
| ***primaryCellMeasuredResults***  This field contains measurements for the primary cell (if the primary cell is a E-UTRA or NB-IoT cell), when the target device reports measurements for both primary cell (E-UTRA or NB-IoT) and neighbour cells. This field shall be omitted when the target device reports measurements for the primary cell (E-UTRA or NB-IoT) only, in which case the measurements for the primary cell (E-UTRA or NB-IoT) is reported in the *measuredResultsList*. This field shall be omitted when the primary cell is not a E-UTRA or NB-IoT cell. |
| ***measuredResultsList***  This list contains the E‑CID measurements for up to 32 E-UTRA or NB-IoT cells. |
| ***physCellId***  This field specifies the physical cell identity of the measured cell. |
| ***cellGlobalId***  This field specifies cell global ID of the measured cell. The target device shall provide this field if it was able to determine the ECGI of the measured cell at the time of measurement. |
| ***arfcnEUTRA***  This field specifies the ARFCN of the measured E-UTRA carrier frequency, as defined in TS 36.331 [12]. In the case the target device includes *arfcnEUTRA-v9a0*, the target device shall set the corresponding *arfcnEUTRA* (i.e. without suffix) to *maxEARFCN*. |
| ***systemFrameNumber***  This field specifies the system frame number of the measured cell during which the measurements have been performed. The target device shall include this field if it was able to determine the SFN of the cell at the time of measurement. |
| ***rsrp-Result***  This field specifies the reference signal received power (RSRP) measurement, as defined in TS 36.331 [12], TS 36.214 [17]. In the case the target device includes *rsrp-Result-v1470*, the target device shall set the corresponding *rsrp-Result* (i.e. without suffix) to value 0. |
| ***rsrq-Result***  This field specifies the reference signal received quality (RSRQ) measurement, as defined in TS 36.331 [12], TS 36.214 [17]. In the case the target device includes *rsrq-Result-v1470*, the target device shall set the corresponding *rsrq-Result* (i.e. without suffix) to value 0 or 34. |
| ***ue-RxTxTimeDiff***  This field specifies the UE Rx–Tx time difference measurement, as defined in TS 36.214 [17]. It is provided only for measurements on the UE's primary cell.  Measurement report mapping is according to TS 36.133 [18]. |
| ***nrsrp-Result***  This field specifies the narrowband reference signal received power (NRSRP) measurement, as defined in TS 36.214 [17]. Measurement report mapping is according to TS 36.133 [18]. |
| ***nrsrq-Result***  This field specifies the narrowband reference signal received quality (NRSRQ) measurement, as defined in TS 36.214 [17].  Measurement report mapping to the value defined in TS 36.133 [18]. Values 0..29 map to values  NRSRQ\_-30..NRSRQ\_-1. Values 30..62 map to NRSRQ\_01..NRSRQ\_33. Values 63..74 map to NRSRQ\_35..NRSRQ\_46. The UE does not report NRSRQ\_00 nor NRSRQ\_34. |
| ***carrierFreqOffsetNB***  This field specifies the offset of the NB-IoT channel number to ARFCN given by *arfcnEUTRA* as defined in TS 36.101 [21]. |
| ***hyperSFN***  This field specifies the hyper-SFN of the measured cell during which the measurements have been performed. The target device shall include this field if it was able to determine the hyper-SFN of the cell at the time of measurement. |

#### 6.5.3.3 E‑CID Location Information Request

#### – *ECID-RequestLocationInformation*

The IE *ECID-RequestLocationInformation* is used by the location server to request E‑CID location measurements from a target device.

-- ASN1START

ECID-RequestLocationInformation ::= SEQUENCE {

requestedMeasurements BIT STRING { rsrpReq (0),

rsrqReq (1),

ueRxTxReq (2),

nrsrpReq-r14 (3),

nrsrqReq-r14 (4)} (SIZE(1..8)),

...

}

-- ASN1STOP

| *ECID-RequestLocationInformation* field descriptions |
| --- |
| ***requestedMeasurements***  This field specifies the E‑CID measurements requested. This is represented by a bit string, with a one‑value at the bit position means the particular measurement is requested; a zero‑value means not requested. |

#### 6.5.3.4 E‑CID Capability Information

#### – *ECID-ProvideCapabilities*

The IE *ECID-ProvideCapabilities* is used by the target device to indicate its capability to support E‑CID and to provide its E‑CID location capabilities to the location server.

-- ASN1START

ECID-ProvideCapabilities ::= SEQUENCE {

ecid-MeasSupported BIT STRING { rsrpSup (0),

rsrqSup (1),

ueRxTxSup (2),

nrsrpSup-r14 (3),

nrsrqSup-r14 (4)} (SIZE(1..8)),

...,

[[ ueRxTxSupTDD-r13 ENUMERATED { true } OPTIONAL

]],

[[ periodicalReporting-r14 ENUMERATED { supported } OPTIONAL,

triggeredReporting-r14 ENUMERATED { supported } OPTIONAL,

idleStateForMeasurements-r14 ENUMERATED { required } OPTIONAL

]],

[[ scheduledLocationRequestSupported-r17 ScheduledLocationTimeSupport-r17 OPTIONAL

]],

[[ periodicReportingIntervalMsSupport-r18 PeriodicReportingIntervalMsSupport-r18 OPTIONAL

]]

}

-- ASN1STOP

| *ECID-Provide-Capabilities* field descriptions |
| --- |
| ***ecid-MeasSupported***  This field specifies the E‑CID measurements supported by the target device. This is represented by a bit string, with a one‑value at the bit position means the particular measurement is supported; a zero‑value means not supported. A zero-value in all bit positions in the bit string means only the basic Cell ID positioning method is supported by the target device.  If the UE Rx-Tx time difference measurement is supported by the target device (i.e., *ueRxTxSup* field is set to one), it means that the UE supports the UE Rx-Tx time difference measurement reporting via both LPP signaling and RRC signalling.  If a target device doesn't support LPP, the E-SMLC may assume the target device can not report the UE Rx-Tx time difference measurement results via RRC signalling. |
| ***ueRxTxSupTDD***  This field, if present, indicates that any UE Rx-Tx time difference measurement reporting for TDD from the target device includes the *NTAoffset*according to TS 36.211 [16], TS 36.214 [17] and uses the UE Rx-Tx time difference measurement report mapping for TDD as specified in TS 36.133 [18]. This field may only be included if the *ueRxTxSup* field in *ecid‑MeasSupported* is set to value one. |
| ***periodicalReporting***  This field, if present, indicates that the target device supports *periodicalReporting* of E-CID measurements*.* If this field is absent, the location server may assume that the target device does not support *periodicalReporting* in *CommonIEsRequestLocationInformation*. |
| ***triggeredReporting***  This field, if present, indicates that the target device supports *triggeredReporting* for the *cellChange* event. If this field is absent, the location server may assume that the target device does not support *triggeredReporting* in *CommonIEsRequestLocationInformation*. |
| ***idleStateForMeasurements***  This field, if present, indicates that the target device requires idle state to perform E-CID measurements. |
| ***scheduledLocationRequestSupported***  This field, if present, indicates that the target device supports scheduled location requests – i.e., supports the IE *ScheduledLocationTime* in IE *CommonIEsRequestLocationInformation* – and the time base(s) supported for the scheduled location time. |
| ***periodicReportingIntervalMsSupport***  This field, if present, indicates that the target device supports millisecond periodic reporting intervals for location information – i.e., supports the subfield *reportingIntervalMs* of the IE *PeriodicalReportingCriteriaExt* in IE *CommonIEsRequestLocationInformation* – and the minimum millisecond report interval supported for the periodic reporting. |

#### 6.5.3.5 E‑CID Capability Information Request

#### – *ECID-RequestCapabilities*

The IE *ECID-RequestCapabilities* is used by the location server to request E‑CID positioning capabilities from a target device.

-- ASN1START

ECID-RequestCapabilities ::= SEQUENCE {

...

}

-- ASN1STOP

#### 6.5.3.6 E‑CID Error Elements

#### – *ECID-Error*

The IE *ECID-Error* is used by the location server or target device to provide E‑CID error reasons to the target device or location server, respectively.

-- ASN1START

ECID-Error ::= CHOICE {

locationServerErrorCauses ECID-LocationServerErrorCauses,

targetDeviceErrorCauses ECID-TargetDeviceErrorCauses,

...

}

-- ASN1STOP

#### – *ECID-LocationServerErrorCauses*

The IE *ECID-LocationServerErrorCauses* is used by the location server to provide E‑CID error reasons to the target device.

-- ASN1START

ECID-LocationServerErrorCauses ::= SEQUENCE {

cause ENUMERATED { undefined,

...

},

...

}

-- ASN1STOP

#### – *ECID-TargetDeviceErrorCauses*

The IE *ECID-TargetDeviceErrorCauses* is used by the target device to provide E-CID error reasons to the location server.

-- ASN1START

ECID-TargetDeviceErrorCauses ::= SEQUENCE {

cause ENUMERATED { undefined,

requestedMeasurementNotAvailable,

notAllrequestedMeasurementsPossible,

...

},

rsrpMeasurementNotPossible NULL OPTIONAL,

rsrqMeasurementNotPossible NULL OPTIONAL,

ueRxTxMeasurementNotPossible NULL OPTIONAL,

...,

[[

nrsrpMeasurementNotPossible-r14 NULL OPTIONAL,

nrsrqMeasurementNotPossible-r14 NULL OPTIONAL

]]

}

-- ASN1STOP

| *ECID-TargetDeviceErrorCauses* field descriptions |
| --- |
| ***cause***  This field provides a E-CID specific error cause. If the cause value is 'notAllRequestedMeasurementsPossible', the target device was not able to provide all requested E-CID measurements (but may be able to provide some measurements). In this case, the target device should include any of the *rsrpMeasurementNotPossible*, *rsrqMeasurementNotPossible*, *ueRxTxMeasurementNotPossible*, *nrsrpMeasurementNotPossible*, or *nrsrqMeasurementNotPossible* fields, as applicable. |

### 6.5.4 Terrestrial Beacon System Positioning

#### 6.5.4.1 TBS Location Information

#### – *TBS-ProvideLocationInformation*

The IE *TBS-ProvideLocationInformation* is used by the target device to provide TBS location measurements to the location server. It may also be used to provide TBS positioning specific error reason.

-- ASN1START

TBS-ProvideLocationInformation-r13 ::= SEQUENCE {

tbs-MeasurementInformation-r13 TBS-MeasurementInformation-r13 OPTIONAL,

tbs-Error-r13 TBS-Error-r13 OPTIONAL,

...

}

-- ASN1STOP

#### 6.5.4.2 TBS Location Information Elements

#### – *TBS-MeasurementInformation*

The IE *TBS-MeasurementInformation* is used by the target device to provide TBS location measurements to the location server.

-- ASN1START

TBS-MeasurementInformation-r13 ::= SEQUENCE {

measurementReferenceTime-r13 UTCTime OPTIONAL,

mbs-SgnMeasList-r13 MBS-BeaconMeasList-r13 OPTIONAL, -- Cond MBS

...

}

-- ASN1STOP

| Conditional presence | Explanation |
| --- | --- |
| *MBS* | The field is mandatory present if the *TBS-MeasurementInformation* is provided for an MBS system; otherwise it is not present. |

| *TBS-MeasurementInformation* field descriptions |
| --- |
| ***measurementReferenceTime***  This field provides the UTC time when the TBS measurements are performed and should take the form of *YYMMDDhhmmssZ*. |
| ***mbs-SgnMeasList***  This field provides the MBS measurements for up to 64 MBS beacons. |

#### – *MBS-BeaconMeasList*

The IE *MBS-BeaconMeasList* is used by the target device to provide MBS location measurements to the location server, as defined in the MBS ICD [24].

-- ASN1START

MBS-BeaconMeasList-r13 ::= SEQUENCE (SIZE(1..64)) OF MBS-BeaconMeasElement-r13

MBS-BeaconMeasElement-r13 ::= SEQUENCE {

transmitterID-r13 INTEGER (0..32767),

codePhase-r13 INTEGER (0..2097151),

codePhaseRMSError-r13 INTEGER (0..63),

...,

[[ rssi-r14 INTEGER (-130..-30) OPTIONAL

]]

}

-- ASN1STOP

| *MBS-BeaconMeasList* field descriptions |
| --- |
| ***transmitterID***  This field contains the MBS transmitter identifier. |
| ***codePhase***  This field contains the value of the code-phase measurement made by the target device for the particular beacon signal at the time of measurement in the units of ms. MBS specific code phase measurements (e.g. chips) are converted into unit of ms by dividing the measurements by the nominal values of the measured signal chipping rate.  Scale factor 2-21 milli‑seconds, in the range from 0 to (1-2-21) milli‑seconds. |
| ***codePhaseRMSError***  This field contains the pseudorange RMS error value. This parameter is specified according to a floating-point representation shown in the table below. |
| ***rssi***  This field provides an estimate of the received signal strength from the MBS beacon as referenced to the UE antenna connector.  If the estimated received signal strength for the MBS beacon is less than -130 dBm, the UE shall report an RSSI value of -130. If the estimated received signal strength for the MBS beacon is greater than -30 dBm, the UE shall report an RSSI value of -30.  Scale factor 1 dBm. |

floating-point representation

| Index | Mantissa | Exponent | Floating-Point value, xi | Pseudorange value, P [m] |
| --- | --- | --- | --- | --- |
| 0 | 000 | 000 | 0.5 | P < 0.5 |
| 1 | 001 | 000 | 0.5625 | 0.5 <= P < 0.5625 |
| i | x | y | 0.5 \* (1 + x/8) \* 2y | xi-1 <= P < xi |
| 62 | 110 | 111 | 112 | 104 <= P < 112 |
| 63 | 111 | 111 | -- | 112 <= P |

#### 6.5.4.3 TBS Location Information Request

#### – *TBS-RequestLocationInformation*

The IE *TBS-RequestLocationInformation* is used by the location server to request location information for TBS-based methods from the target device.

-- ASN1START

TBS-RequestLocationInformation-r13 ::= SEQUENCE {

mbsSgnMeasListReq-r13 BOOLEAN,

...,

[[ mbsAssistanceAvailability-r14 BOOLEAN OPTIONAL, -- Need ON

mbsRequestedMeasurements-r14 BIT STRING {

rssi (0)} (SIZE(1..8)) OPTIONAL -- Need ON

]]

}

-- ASN1STOP

| *TBS-RequestLocationInformation* field descriptions |
| --- |
| ***mbsSgnMeasListReq***  This field indicates whether the target device is requested to report MBS measurements in *TBS‑MeasurementInformation* IE or not. TRUE means requested. |
| ***mbsAssistanceAvailability***  This field indicates whether the target device may request additional MBS assistance data from the server. TRUE means allowed and FALSE means not allowed. |
| ***mbsRequestedMeasurements***  This field indicates the additional MBS measurements requested and may only be included if *mbsSgnMeasListReq* is set to TRUE. This field is represented by a bit string, with a one‑value at the bit position means the particular measurement is requested; a zero‑value means not requested. The following measurement requests can be included.  rssi: Beacon signal strength at the target |

#### 6.5.4.4 TBS Capability Information

#### – *TBS-ProvideCapabilities*

The IE *TBS-ProvideCapabilities* is used by the target device to indicate its capability to support TBS and to provide its TBS location capabilities to the location server.

-- ASN1START

TBS-ProvideCapabilities-r13 ::= SEQUENCE {

tbs-Modes-r13 BIT STRING { standalone (0),

ue-assisted (1),

ue-based (2)} (SIZE (1..8)),

...,

[[ mbs-AssistanceDataSupportList-r14 MBS-AssistanceDataSupportList-r14 OPTIONAL,

periodicalReportingSupported-r14 PositioningModes OPTIONAL,

mbs-ConfigSupport-r14 BIT STRING { tb1 (0),

tb2 (1),

tb3 (2),

tb4 (3)} (SIZE (1..8)) OPTIONAL,

mbs-IdleStateForMeasurements-r14 ENUMERATED { required } OPTIONAL

]],

[[ scheduledLocationRequestSupported-r17 ScheduledLocationTimeSupportPerMode-r17 OPTIONAL

]],

[[ periodicReportingIntervalMsSupport-r18 PeriodicReportingIntervalMsSupportPerMode-r18

OPTIONAL

]]

}

-- ASN1STOP

| *TBS-ProvideCapabilities* field descriptions |
| --- |
| ***tbs-Modes***  This field specifies the TBS mode(s) supported by the target device. This is represented by a bit string, with a one‑value at the bit position means the particular TBS mode is supported; a zero‑value means not supported. |
| ***mbs-AssistanceDataSupportList***  This list defines the MBS assistance data supported by the target device. This field shall be present if the target device supports MBS assistance data. |
| ***periodicalReportingSupported***  This field, if present, specifies the positioning modes for which the target device supports *periodicalReporting.* This is represented by a bit string, with a one‑value at the bit position means *periodicalReporting* for the positioning mode is supported; a zero‑value means not supported. If this field is absent, the location server may assume that the target device does not support *periodicalReporting* in *CommonIEsRequestLocationInformation*. |
| ***mbs-ConfigSupport***  This field specifies the MBS configurations supported by the target device. This field shall be present if the target device supports MBS [24]. |
| ***mbs-IdleStateForMeasurements***  This field, if present, indicates that the target device requires idle state to perform MBS measurements. |
| ***scheduledLocationRequestSupported***  This field, if present, specifies the positioning modes for which the target device supports scheduled location requests – i.e., supports the IE *ScheduledLocationTime* in IE *CommonIEsRequestLocationInformation* – and the time base(s) supported for the scheduled location time for each positioning mode. If this field is absent, the target device does not support scheduled location requests. |
| ***periodicReportingIntervalMsSupport***  This field, if present, specified the supported minimum millisecond periodic reporting interval for location information per positioning mode – i.e., supports the subfield *reportingIntervalMs* of the IE *PeriodicalReportingCriteriaExt* in IE *CommonIEsRequestLocationInformation* – and the minimum millisecond report interval supported for the periodic reporting. |

#### *- MBS-AssistanceDataSupportList*

The IE *MBS-AssistanceDataSupportList* is used by the target device to indicate its capability to support MBS Assistance Data and to provide its capabilities to the location server.

-- ASN1START

MBS-AssistanceDataSupportList-r14 ::= SEQUENCE {

mbs-AcquisitionAssistanceDataSupport-r14 BOOLEAN,

mbs-AlmanacAssistanceDataSupport-r14 BOOLEAN,

...

}

-- ASN1STOP

| *MBS-AssistanceDataSupportList* field descriptions |
| --- |
| ***mbs-AcquisitionAssistanceDataSupport***  This field specifies whether the target device supports MBS Acquisition Assistance Data. TRUE means supported. |
| ***mbs-AlmanacAssistanceDataSupport***  This field specifies whether the target device supports MBS Almanac Assistance Data. TRUE means supported. |

#### 6.5.4.5 TBS Capability Information Request

#### – *TBS-RequestCapabilities*

The IE *TBS-RequestCapabilities* is used by the location server to request TBS positioning capabilities from a target device.

-- ASN1START

TBS-RequestCapabilities-r13 ::= SEQUENCE {

...

}

-- ASN1STOP

#### 6.5.4.6 TBS Error Elements

#### – *TBS-Error*

The IE *TBS-Error* is used by the location server or target device to provide TBS error reasons to the target device or location server, respectively.

-- ASN1START

TBS-Error-r13 ::= CHOICE {

locationServerErrorCauses-r13 TBS-LocationServerErrorCauses-r13,

targetDeviceErrorCauses-r13 TBS-TargetDeviceErrorCauses-r13,

...

}

-- ASN1STOP

#### – *TBS-LocationServerErrorCauses*

The IE *TBS-LocationServerErrorCauses* is used by the location server to provide error reasons for TBS positioning to the target device.

-- ASN1START

TBS-LocationServerErrorCauses-r13 ::= SEQUENCE {

cause-r13 ENUMERATED { undefined,

...,

assistanceDataNotSupportedByServer-v1420,

assistanceDataSupportedButCurrentlyNotAvailableByServer-v1420

},

...

}

-- ASN1STOP

#### – *TBS-TargetDeviceErrorCauses*

The IE *TBS-TargetDeviceErrorCauses* is used by the target device to provide error reasons for TBS positioning to the location server.

-- ASN1START

TBS-TargetDeviceErrorCauses-r13 ::= SEQUENCE {

cause-r13 ENUMERATED { undefined,

thereWereNotEnoughMBSBeaconsReceived,

...,

assistanceDataMissing-v1420

},

...

}

-- ASN1STOP

| *TBS-TargetDeviceErrorCauses* field descriptions |
| --- |
| ***cause***  This field provides a TBS specific error cause. |

#### 6.5.4.7 TBS Assistance Data

#### – *TBS-ProvideAssistanceData*

The IE *TBS-ProvideAssistanceData* is used by the location server to provide assistance data to assist in position estimation at the UE (e.g. for UE‑based mode) and/or to expedite the acquisition of TBS signals. It may also be used to provide TBS positioning specific error reasons.

-- ASN1START

TBS-ProvideAssistanceData-r14 ::= SEQUENCE {

tbs-AssistanceDataList-r14 TBS-AssistanceDataList-r14 OPTIONAL, -- Need ON

tbs-Error-r14 TBS-Error-r13 OPTIONAL, -- Need ON

...

}

-- ASN1STOP

#### 6.5.4.8 TBS Assistance Data Elements

#### – *TBS-AssistanceDataList*

The IE *TBS-AssistanceDataList* is used by the location server to provide the TBS specific assistance data to the UE.

-- ASN1START

TBS-AssistanceDataList-r14 ::= SEQUENCE {

mbs-AssistanceDataList-r14 MBS-AssistanceDataList-r14 OPTIONAL, -- Need ON

...

}

MBS-AssistanceDataList-r14 ::= SEQUENCE (SIZE (1..maxMBS-r14)) OF MBS-AssistanceDataElement-r14

MBS-AssistanceDataElement-r14 ::= SEQUENCE {

mbs-AlmanacAssistance-r14 MBS-AlmanacAssistance-r14 OPTIONAL, -- Need ON

mbs-AcquisitionAssistance-r14 MBS-AcquisitionAssistance-r14 OPTIONAL, -- Need ON

...

}

-- ASN1STOP

#### – *MBS-AlmanacAssistance*

The IE *MBS-AlmanacAssistance* is used by the location server to provide LLA of MBS transmitters to enable position estimation at the UE.

-- ASN1START

MBS-AlmanacAssistance-r14 ::= SEQUENCE {

transmitterID-r14 INTEGER (0..32767),

transmitterLatitude-r14 BIT STRING (SIZE (26)),

transmitterLongitude-r14 BIT STRING (SIZE (27)),

transmitterAltitude-r14 BIT STRING (SIZE (15)),

timeCorrection-r14 INTEGER (0..25) OPTIONAL, -- Need ON

...

}

-- ASN1STOP

| *MBS-AlmanacAssistance* field descriptions |
| --- |
| ***transmitterID***  This field specifies the MBS transmitter ID [24]. |
| ***transmitterLatitude***  This field specifies latitude of the MBS transmitter, degrees. Scale factor 4/220 decimal degrees, added to -90°. Valid range -90° to 90° [24]. |
| ***transmitterLongitude***  This field specifies longitude of the MBS transmitter, degrees. Scale factor 4/220 decimal degrees, added to -180°. Valid range -180° to 180° [24]. |
| ***transmitterAltitude***  This field specifies altitude of the MBS transmitter, metres. Scale factor 0.29 metres, added to -500 metres.  Valid range -500 to 9002.43 metres [24]. |
| ***timeCorrection***  This field contains the residual timing error for a particular beacon, in units of nano-seconds, in the range from 0 to 25. This field is used for UE-based mode only, by subtracting from the *codePhase* measurement made by the target device [24]. |

#### – *MBS-AcquisitionAssistance*

The IE *MBS-AcquisitionAssistance* is used by the location server to provide parameters that support acquisition of the MBS signals [24].

-- ASN1START

MBS-AcquisitionAssistance-r14 ::= SEQUENCE {

transmitterID-r14 INTEGER (0..32767) OPTIONAL, -- Need ON

mbsConfiguration-r14 ENUMERATED {tb1, tb2, tb3, tb4, ...} OPTIONAL, -- Need ON

pnCodeIndex-r14 INTEGER (1..128) OPTIONAL, -- Need ON

freq-r14 INTEGER (919750000..927250000) OPTIONAL, -- Need ON

...

}

-- ASN1STOP

| *MBS-AcquisitionAssistance* field descriptions |
| --- |
| ***transmitterID***  This field contains the MBS transmitter identifier [24]. |
| ***mbsConfiguration***  This field specifies MBS configuration as defined in the MBS ICD [24]. |
| ***pnCodeIndex***  This field specifies the index of the MBS PN code [24]. |
| ***freq***  This field specifies the MBS signal centre frequency in units of Hz [24]. |

#### 6.5.4.9 TBS Assistance Data Request

#### – *TBS-RequestAssistanceData*

The IE *TBS-RequestAssistanceData* is used by the target device to request TBS assistance data from a location server.

-- ASN1START

TBS-RequestAssistanceData-r14 ::= SEQUENCE {

mbs-AlmanacAssistanceDataReq-r14 BOOLEAN,

mbs-AcquisitionAssistanceDataReq-r14 BOOLEAN,

...

}

-- ASN1STOP

### 6.5.5 Sensor based Positioning

#### 6.5.5.0 Introduction

This clause defines support for sensor-based positioning. The supported sensor methods are "Barometric pressure sensor" and "Motion sensor" as described in TS 36.305, clauses 8.6 and 8.10 respectively [2].

#### 6.5.5.1 Sensor Location Information

#### – *Sensor-ProvideLocationInformation*

The IE *Sensor-ProvideLocationInformation* is used by the target device to provide location information for sensor-based methods to the location server. It may also be used to provide sensor specific error reason.

-- ASN1START

Sensor-ProvideLocationInformation-r13 ::= SEQUENCE {

sensor-MeasurementInformation-r13 Sensor-MeasurementInformation-r13 OPTIONAL,

sensor-Error-r13 Sensor-Error-r13 OPTIONAL,

...,

[[

sensor-MotionInformation-r15 Sensor-MotionInformation-r15 OPTIONAL

]]

}

-- ASN1STOP

#### 6.5.5.2 Sensor Location Information Elements

#### – *Sensor-MeasurementInformation*

The IE *Sensor-MeasurementInformation* is used by the target device to provide UE sensor measurements to the location server.

-- ASN1START

Sensor-MeasurementInformation-r13 ::= SEQUENCE {

measurementReferenceTime-r13 UTCTime OPTIONAL,

uncompensatedBarometricPressure-r13 INTEGER (30000..115000) OPTIONAL, -- Cond Barometer

...,

[[

uncertainty-r14 SEQUENCE {

range-r14 INTEGER (0..1000),

confidence-r14 INTEGER (1..100)

} OPTIONAL

]],

[[ adjustment-r16 INTEGER (-5000..5000) OPTIONAL

]]

}

-- ASN1STOP

| Conditional presence | Explanation |
| --- | --- |
| *Barometer* | The field is mandatory present if the *Sensor-MeasurementInformation* is provided for barometric pressure; otherwise it is not present. |

| *Sensor-MeasurementInformation* field descriptions |
| --- |
| ***measurementReferenceTime***  This field provides the UTC time when the sensor measurements are performed and should take the form of *YYMMDDhhmmssZ.* |
| ***uncompensatedBarometricPressure***  This field provides the uncompensated barometric pressure as measured by the UE sensor, in units of Pa. |
| ***uncertainty***  This field provides the expected range for the pressure measurement in units of Pa and the confidence as a percentage that the true pressure lies in a range of (measurement – range) to (measurement + range). |
| ***adjustment***  This field provides any adjustment available in the UE, in units of Pa, to allow the production of a compensated atmospheric pressure measurement where compensated atmospheric pressure = *uncompensatedBarometricPressure* + *adjustment* |

#### – *Sensor-MotionInformation*

The IE *Sensor-MotionInformation* is used by the target device to provide UE movement information to the location server. The movement information comprises an ordered series of points. This information may be obtained by the target device using one or more motion sensors.

-- ASN1START

Sensor-MotionInformation-r15 ::= SEQUENCE {

refTime-r15 DisplacementTimeStamp-r15,

displacementInfoList-r15 DisplacementInfoList-r15,

...

}

DisplacementInfoList-r15 ::= SEQUENCE (SIZE (1..128)) OF DisplacementInfoListElement-r15

DisplacementInfoListElement-r15 ::= SEQUENCE {

deltaTimeStamp-r15 DeltaTime-r15,

displacement-r15 Displacement-r15 OPTIONAL,

...

}

DisplacementTimeStamp-r15 ::= CHOICE {

utcTime-r15 UTC-Time-r15,

gnssTime-r15 MeasurementReferenceTime,

systemFrameNumber-r15 SFN-r15,

measurementSFN-r15 INTEGER(-8192..9214),

...

}

DeltaTime-r15 ::= CHOICE {

deltaTimeSec-r15 INTEGER (1..16384),

deltaTimeSFN-r15 INTEGER (1..4096),

...

}

SFN-r15 ::= SEQUENCE {

sfn-r15 BIT STRING (SIZE (10)),

hyperSFN-r15 BIT STRING (SIZE (10)) OPTIONAL,

...

}

Displacement-r15 ::= SEQUENCE {

bearing-r15 INTEGER (0..3599),

bearingUncConfidence-r15 INTEGER (0..100) OPTIONAL,

bearingRef-r15 ENUMERATED { geographicNorth, magneticNorth, local },

horizontalDistance-r15 INTEGER (0..8191),

horizontalDistanceUnc-r15 INTEGER (0..255) OPTIONAL,

horizontalUncConfidence-r15 INTEGER (0..100) OPTIONAL,

verticalDirection-r15 ENUMERATED{upward, downward} OPTIONAL,

verticalDistance-r15 INTEGER(0..8191) OPTIONAL,

verticalDistanceUnc-r15 INTEGER (0..255) OPTIONAL,

verticalUncConfidence-r15 INTEGER (0..100) OPTIONAL,

...

}

UTC-Time-r15 ::= SEQUENCE {

utcTime-r15 UTCTime,

utcTime-ms-r15 INTEGER (0..999),

...

}

-- ASN1STOP

| *Sensor-MotionInformation* field descriptions |
| --- |
| ***refTime***  This field provides the reference time *t0* associated with the starting position of the first displacement in the displacement list. |
| ***displacementInfoList***  This field provides an ordered series of direction and distance travelled by the target device and comprises the following subfields:  - ***deltaTimeStamp*** specifies the time between *tn-1* and *tn*, were *n* corresonds to the order of entry in the *DispacementInfoList* (*n*=0 correspond to the time provided in *refTime*).  - ***displacement*** provides the direction and distance travelled between time *tn-1* and *tn*. |
| ***utcTime***  This field provides the time stamp of the *refTime* in UTC time and comprises the following subfields:  - *utcTime* in the form of YYMMDDhhmmssZ.  - *utcTime-ms* specifies the fractional part of the UTC time in ms resolution. |
| ***gnssTime***  This field provides the time stamp of the *refTime* in GNSS time. |
| ***systemFrameNumber***  This field provides the time stamp of the *refTime* in serving cell SFN time. |
| ***measurementSFN***  This field provides the time stamp of the *refTime* in form of the measurement SFN as defined in *delta-SFN* in IE *OTDOA-SignalMeasurementInformation*. This field may be included when OTDOA measurements are included. |
| ***deltaTimeSec***  This field provides the time between *tn-1* and *tn* in units of milliseconds. |
| ***deltaTimeSFN***  This field provides the time between *tn-1* and *tn* in units of system frame numbers. |
| ***bearing***  This field specifies the direction (heading) of the horizontal displacement measured clockwise from *bearingRef*.  Scale factor 0.1 degree. |
| ***bearingRef***  This field specifies the reference direction for the *bearing*. Enumerated value '*geographicNorth*' indicates that the *bearing* is measured clockwise from the Geographic North; '*magneticNorth*' indicates that the *bearing* is measured clockwise from the Magnetic North; '*local*' indicates that the *bearing* is measured clockwise from an arbitrary (undefined) reference direction. |
| ***horizontalDistance***  This field specifies the horizonal distance travelled between time *tn-1* and *tn*.  Scale factor 1 cm. |
| ***horizontalDistanceUnc, horizontalUncConfidence***  This field specifies the horizontal uncertainty of the displacement (corresponding to *tn*). *horizontalDistanceUnc* correspond to the encoded high accuracy uncertainty as defined in TS 23.032 [15]*. horizontalUncConfidence* corresponds to confidence as defined in TS 23.032 [15]. |
| ***verticalDistance***  This field specifies the vertical distance travelled between time *tn-1* and *tn*.  Scale factor 1 cm. |
| ***verticalDistanceUnc, verticalUncConfidence***  This field specifies the vertical uncertainty of the displacement (corresponding to *tn*). *verticalDistanceUnc* correspond to the encoded high accuracy uncertainty as defined in TS 23.032 [15]. *verticalUncConfidence* corresponds to confidence as defined in TS 23.032 [15]. |

#### 6.5.5.3 Sensor Location Information Request

#### – *Sensor-RequestLocationInformation*

The IE *Sensor-RequestLocationInformation* is used by the location server to request location information for sensor-based methods from a target device.

-- ASN1START

Sensor-RequestLocationInformation-r13 ::= SEQUENCE {

uncompensatedBarometricPressureReq-r13 BOOLEAN,

...,

[[ assistanceAvailability-r14 BOOLEAN OPTIONAL -- Need ON

]],

[[ sensor-MotionInformationReq-r15 BOOLEAN OPTIONAL -- Need ON

]],

[[ adjustmentReq-r16 BOOLEAN OPTIONAL -- Need ON

]]

}

-- ASN1STOP

| *Sensor-RequestLocationInformation* field descriptions |
| --- |
| ***uncompensatedBarometricPressureReq***  This field indicates whether the target device is requested to report Barometric pressure measurements in *Sensor‑MeasurementInformation* IE or not. TRUE means requested. |
| ***assistanceAvailability***  This field indicates whether the target device may request additional Sensor assistance data from the server. TRUE means allowed and FALSE means not allowed. |
| ***sensor-MotionInformationReq***  This field indicates whether the target device is requested to report movement information in IE *Sensor‑MotionInformation* or not. TRUE means requested. |
| ***adjustmentReq***  This field indicates whether the target device is requested to report *adjustment* in IE *Sensor-MeasurementInformation* or not. TRUE means requested. |

#### 6.5.5.4 Sensor Capability Information

#### *– Sensor-ProvideCapabilities*

The IE *Sensor-ProvideCapabilities* is used by the target device to provide capabilities for sensor-based methods from to the location server.

-- ASN1START

Sensor-ProvideCapabilities-r13 ::= SEQUENCE {

sensor-Modes-r13 BIT STRING { standalone (0),

ue-assisted (1),

ue-based (2)} (SIZE (1..8)),

...,

[[ sensor-AssistanceDataSupportList-r14 Sensor-AssistanceDataSupportList-r14 OPTIONAL,

periodicalReportingSupported-r14 PositioningModes OPTIONAL,

idleStateForMeasurements-r14 ENUMERATED { required } OPTIONAL

]],

[[ sensor-MotionInformationSup-r15 ENUMERATED { true } OPTIONAL

]],

[[ adjustmentSupported-r16 ENUMERATED { true } OPTIONAL

]],

[[ scheduledLocationRequestSupported-r17 ScheduledLocationTimeSupportPerMode-r17 OPTIONAL

]],

[[ periodicReportingIntervalMsSupport-r18 PeriodicReportingIntervalMsSupportPerMode-r18

OPTIONAL

]]

}

Sensor-AssistanceDataSupportList-r14 ::= SEQUENCE {

...,

[[ validityPeriodSupported-v1520 ENUMERATED { true } OPTIONAL,

validityAreaSupported-v1520 ENUMERATED { true } OPTIONAL

]]

}

-- ASN1STOP

| *Sensor-ProvideCapabilities* field descriptions |
| --- |
| ***sensor-Modes***  This field specifies the sensor mode(s) supported by the target device. This is represented by a bit string, with a one‑value at the bit position means the particular sensor mode is supported; a zero‑value means not supported. |
| ***sensor-AssistanceDataSupportList***  This field specifies a list of sensor assistance data supported by the target device. This field shall be present if the target device supports assistance data for Barometric pressure sensor. |
| ***validityPeriodSupported***  This field, if present, indicates that the target device supports *period* i.e. pressure validity period and pressure rate as part of the *Sensor-AssistanceDataList*. |
| ***valitidyAreaSupported***  This field, if present, indicates that the target device supports *area* i.e. pressure validity area and North/East pressure gradient as part of the *Sensor-AssistanceDataList*. |
| ***periodicalReportingSupported***  This field, if present, specifies the positioning modes for which the target device supports *periodicalReporting.* This is represented by a bit string, with a one‑value at the bit position means *periodicalReporting* for the positioning mode is supported; a zero‑value means not supported. If this field is absent, the location server may assume that the target device does not support *periodicalReporting* in *CommonIEsRequestLocationInformation*. |
| ***idleStateForMeasurements***  This field, if present, indicates that the target device requires idle state to perform sensor measurements. |
| ***sensor-MotionInformationSup***  This field, if present, indicates that the target device supports displacement reporting in IE *Sensor-MotionInformation*. |
| ***adjustmentSupported***  This field, if present, indicates that the target device supports the *adjustment* IE in *Sensor-MeasurementInformation*. |
| ***scheduledLocationRequestSupported***  This field, if present, specifies the positioning modes for which the target device supports scheduled location requests – i.e., supports the IE *ScheduledLocationTime* in IE *CommonIEsRequestLocationInformation* – and the time base(s) supported for the scheduled location time for each positioning mode. If this field is absent, the target device does not support scheduled location requests. |
| ***periodicReportingIntervalMsSupport***  This field, if present, specified the supported minimum millisecond periodic reporting interval for location information per positioning mode – i.e., supports the subfield *reportingIntervalMs* of the IE *PeriodicalReportingCriteriaExt* in IE *CommonIEsRequestLocationInformation* – and the minimum millisecond report interval supported for the periodic reporting. |

#### 6.5.5.5 Sensor Capability Information Request

#### *– Sensor-RequestCapabilities*

The IE *Sensor-RequestCapabilities* is used by the location server to request capabilities for sensor-based methods from the target device.

-- ASN1START

Sensor-RequestCapabilities-r13 ::= SEQUENCE {

...

}

-- ASN1STOP

#### 6.5.5.6 Sensor Error Elements

#### *–* *Sensor-Error*

The IE *Sensor-Error* is used by the location server or target device to provide Sensor Error Reasons to the target device or location server, respectively.

-- ASN1START

Sensor-Error-r13 ::= CHOICE {

locationServerErrorCauses-r13 Sensor-LocationServerErrorCauses-r13,

targetDeviceErrorCauses-r13 Sensor-TargetDeviceErrorCauses-r13,

...

}

-- ASN1STOP

#### *–* *Sensor-LocationServerErrorCauses*

The IE *Sensor-LocationServerErrorCauses* is used by the location server to provide error reasons for Sensor positioning to the target device.

-- ASN1START

Sensor-LocationServerErrorCauses-r13 ::= SEQUENCE {

cause-r13 ENUMERATED { undefined,

...,

assistanceDataNotSupportedByServer-v1420,

assistanceDataSupportedButCurrentlyNotAvailableByServer-v1420

},

...

}

-- ASN1STOP

#### *–* *Sensor-TargetDeviceErrorCauses*

The IE *Sensor-TargetDeviceErrorCauses* is used by the target device to provide error reasons for Sensor positioning to the location server.

-- ASN1START

Sensor-TargetDeviceErrorCauses-r13 ::= SEQUENCE {

cause-r13 ENUMERATED { undefined,

...,

assistanceDataMissing-v1420

},

...

}

-- ASN1STOP

#### 6.5.5.7 Sensor Assistance Data

#### – *Sensor-ProvideAssistanceData*

The IE *Sensor-ProvideAssistanceData* is used by the location server to provide assistance data to assist in altitude computation at the UE (e.g. for UE‑based mode). It may also be used to provide Sensor positioning specific error reasons.

-- ASN1START

Sensor-ProvideAssistanceData-r14 ::= SEQUENCE {

sensor-AssistanceDataList-r14 Sensor-AssistanceDataList-r14 OPTIONAL, -- Need ON

sensor-Error-r14 Sensor-Error-r13 OPTIONAL, -- Need ON

...

}

-- ASN1STOP

#### 6.5.5.8 Sensor Assistance Data Elements

#### – *Sensor-AssistanceDataList*

The IE *Sensor-AssistanceDataList* is used by the location server to provide the Sensor specific assistance data to the UE.

-- ASN1START

Sensor-AssistanceDataList-r14::= SEQUENCE {

refPressure-r14 INTEGER (-20000..10000),

refPosition-r14 EllipsoidPointWithAltitudeAndUncertaintyEllipsoid OPTIONAL, -- Need ON

refTemperature-r14 INTEGER (-64..63) OPTIONAL, -- Need ON

...,

[[

period-v1520 SEQUENCE {

pressureValidityPeriod-v1520 PressureValidityPeriod-v1520,

referencePressureRate-v1520 INTEGER (-128..127) OPTIONAL, -- Need ON

...

} OPTIONAL, -- Need ON

area-v1520 SEQUENCE {

pressureValidityArea-v1520 PressureValidityArea-v1520,

gN-pressure-v1520 INTEGER (-1024..1023) OPTIONAL, -- Need ON

gE-pressure-v1520 INTEGER (-1024..1023) OPTIONAL, -- Need ON

...

} OPTIONAL -- Need ON

]]

}

PressureValidityArea-v1520 ::= SEQUENCE {

centerPoint-v1520 Ellipsoid-Point,

validityAreaWidth-v1520 INTEGER (1..128),

validityAreaHeight-v1520 INTEGER (1..128),

...

}

PressureValidityPeriod-v1520 ::= SEQUENCE {

beginTime-v1520 GNSS-SystemTime,

beginTimeAlt-v1520 INTEGER (0..2881) OPTIONAL, -- Need ON

duration-v1520 INTEGER (1..2881),

...

}

-- ASN1STOP

| *Sensor-AssistanceDataList* field descriptions |
| --- |
| ***refPressure***  This field specifies the atmospheric pressure (Pa) nominal at sea level, EGM96 [29] to the target.  The scale factor is 1 Pa. The value is added to the nominal pressure of 101325 Pa. |
| ***refPosition***  This field specifies the reference position at which the pressure measurement is made, as an ellipsoid point with altitude and uncertainty ellipsoid. |
| ***refTemperature***  Local temperature measurement at the reference where the pressure measurement is made.  The scale factor 1K. The value is added to 273K. |
| ***period***  This field specifies the pressure validity period and reference pressure rate. |
| ***pressureValidityPeriod***  - ***beginTime***: this field specifies the start time of the pressure validity period in *GNSS System Time*.  - ***beginTimeAlt***: this field specifies an alternative start time. It may be used by the target device if *GNSS-System Time* is not available. The alternative start time is relative to the time the message was received. The scale factor is 15 min. The range is from 0 minutes to 43215 minutes = 30 days.  - ***duration***: this field specifies the duration of the validity period after the begin time. The scale factor is 15 minutes. The range is from 15 minutes to 43215 minutes = 30 days. |
| ***referencePressureRate***  This field specifies the rate of change of pressure. When this field is included, the reference pressure applies only at the start of the pressure validity period. The scale factor is 10Pa/hour. |
| ***area***  This field specifies the area within which the provided atmospheric reference pressure is valid and any spatial drift. |
| ***pressureValidityArea***  - ***centerPoint***: this field specifies the coordinates of the centre of the rectangular validity area.  - ***validityAreaWidth***: this field specifies the width of the rectangular validity area. Width is measured from the centre along the latitude and is measured as the total width of the rectangle. The scale factor is 1km. The range is from 1km to 128km.  - ***validityAreaHeight***: this fields specifies the height of the rectangular validity area. Height is measured from the centre along the longitude and is measured as the total height of the rectangle. The scale factor is 1km. The range is from 1km to 128km.  If this field is present, *refPosition* should not be provided by the location server and if provided, shall be ignored by the target device. |
| ***gN-pressure***  This field specifies the northward gradient of the reference pressure calculated from the centre of the *pressureValidityArea*. The scale factor is 1 Pa/km. If this field is not provided, the gradient is assumed to be zero. |
| ***gE-pressure***  This field specifies the eastward gradient of the reference pressure calculated from the centre of the *pressureValidityArea*. The scale factor is 1 Pa/km. If this field is not provided, the gradient is assumed to be zero. |

#### 6.5.5.9 Sensor Assistance Data Request

#### – *Sensor-RequestAssistanceData*

The IE *Sensor-RequestAssistanceData* is used by the target device to request Sensor assistance data from a location server.

-- ASN1START

Sensor-RequestAssistanceData-r14 ::= SEQUENCE {

...

}

-- ASN1STOP

### 6.5.6 WLAN-based Positioning

This clause defines support for positioning using measurements related to WLAN access points.

#### 6.5.6.1 WLAN Location Information

#### *–* *WLAN-ProvideLocationInformation*

The IE *WLAN-ProvideLocationInformation* is used by the target device to provide measurements for one or more WLANs to the location server. It may also be used to provide WLAN positioning specific error reason.

-- ASN1START

WLAN-ProvideLocationInformation-r13 ::= SEQUENCE {

wlan-MeasurementInformation-r13 WLAN-MeasurementInformation-r13 OPTIONAL,

wlan-Error-r13 WLAN-Error-r13 OPTIONAL,

...

}

-- ASN1STOP

#### 6.5.6.2 WLAN Location Information Elements

#### *–* *WLAN-MeasurementInformation*

-- ASN1START

WLAN-MeasurementInformation-r13 ::= SEQUENCE {

measurementReferenceTime-r13 UTCTime OPTIONAL,

wlan-MeasurementList-r13 WLAN-MeasurementList-r13 OPTIONAL,

...

}

WLAN-MeasurementList-r13 ::= SEQUENCE (SIZE(1..maxWLAN-AP-r13)) OF WLAN-MeasurementElement-r13

WLAN-MeasurementElement-r13 ::= SEQUENCE {

wlan-AP-Identifier-r13 WLAN-AP-Identifier-r13,

rssi-r13 INTEGER (-127..128) OPTIONAL,

rtt-r13 WLAN-RTT-r13 OPTIONAL,

apChannelFrequency-r13 INTEGER (0..256) OPTIONAL,

servingFlag-r13 BOOLEAN OPTIONAL,

...

}

WLAN-AP-Identifier-r13 ::= SEQUENCE {

bssid-r13 OCTET STRING (SIZE (6)),

ssid-r13 OCTET STRING (SIZE (1..32)) OPTIONAL,

...

}

WLAN-RTT-r13 ::= SEQUENCE {

rttValue-r13 INTEGER (0..16777215),

rttUnits-r13 ENUMERATED { microseconds,

hundredsofnanoseconds,

tensofnanoseconds,

nanoseconds,

tenthsofnanoseconds,

... },

rttAccuracy-r13 INTEGER (0..255) OPTIONAL,

...

}

-- ASN1STOP

| *WLAN-MeasurementInformation* field descriptions |
| --- |
| ***measurementReferenceTime***  This field provides the UTC time when the WLAN measurements are performed and should take the form of *YYMMDDhhmmssZ*. |
| ***wlan-MeasurementList***  This field provides the WLAN measurements for up to 64 WLAN APs. |
| ***wlan-AP-Identifier***  This field provides the BSSID and optionally the SSID of the wireless network served by the WLAN AP [26]. |
| ***rssi***  This field provides the AP signal strength (RSSI) of a beacon frame, probe response frame or measurement pilot frame measured at the target in dBm as defined in Table 6-7 of [26]. |
| ***rtt***  This field provides the measured round trip time between the target device and WLAN AP and optionally the accuracy expressed as the standard deviation of the delay. Units for each of these are 1000ns, 100ns, 10ns, 1ns, and 0.1ns. |
| ***apChannelFrequency***  This field provides the AP channel number identification of the reported WLAN AP. |
| ***servingFlag***  This parameter indicates whether a set of WLAN AP measurements were obtained for a serving WLAN AP (TRUE) or a non-serving WLAN AP (FALSE). A target device with multiple radio support may indicate more than one type of serving access for the same time instant. |
| ***rttValue***  This field specifies the Round Trip Time (RTT) measurement between the target device and WLAN AP in units given by the field *rttUnits*. |
| ***rttUnits***  This field specifies the Units for the fields *rttValue* and *rttAccuracy****.*** The available Units are 1000ns, 100ns, 10ns, 1ns, and 0.1ns. |
| ***rttAccuracy***  This field provides the estimated accuracy of the provided *rttValue* expressed as the standard deviation in units given by the field *rttUnits*. |

#### 6.5.6.3 WLAN Location Information Request

#### *–* *WLAN-RequestLocationInformation*

The IE *WLAN-RequestLocationInformation* is used by the location server to request WLAN measurements from a target device.

-- ASN1START

WLAN-RequestLocationInformation-r13 ::= SEQUENCE {

requestedMeasurements-r13 BIT STRING {

rssi (0),

rtt (1)} (SIZE(1..8)),

...,

[[ assistanceAvailability-r14 BOOLEAN OPTIONAL -- Need ON

]]

}

-- ASN1STOP

| *WLAN-RequestLocationInformation* field descriptions |
| --- |
| ***requestedMeasurements***  This field specifies the WLAN measurements requested. This is represented by a bit string, with a one‑value at the bit position means the particular measurement is requested; a zero‑value means not requested. The following measurement requests can be included.  rssi: AP signal strength at the target  rtt: Round Trip Time between target and AP |
| ***assistanceAvailability***  This field indicates whether the target device may request additional WLAN assistance data from the server. TRUE means allowed and FALSE means not allowed. |

#### 6.5.6.4 WLAN Capability Information

#### *–* *WLAN-ProvideCapabilities*

The IE *WLAN-ProvideCapabilites* is used by the target device to provide its capabilities for WLAN positioning to the location server.

-- ASN1START

WLAN-ProvideCapabilities-r13 ::= SEQUENCE {

wlan-Modes-r13 BIT STRING { standalone (0),

ue-assisted (1),

ue-based (2)} (SIZE (1..8)),

wlan-MeasSupported-r13 BIT STRING {

rssi-r13 (0),

rtt-r13 (1)} (SIZE(1..8)),

... ,

[[ wlan-AP-AD-Supported-r14

BIT STRING { ap-identifier (0),

ap-location (1)} (SIZE (1..8))

OPTIONAL,

periodicalReportingSupported-r14 PositioningModes OPTIONAL,

idleStateForMeasurements-r14

ENUMERATED { required } OPTIONAL

]],

[[ scheduledLocationRequestSupported-r17 ScheduledLocationTimeSupportPerMode-r17 OPTIONAL

]],

[[ periodicReportingIntervalMsSupport-r18 PeriodicReportingIntervalMsSupportPerMode-r18

OPTIONAL

]]

}

-- ASN1STOP

| *WLAN-ProvideCapabilities* field descriptions |
| --- |
| ***wlan-Modes***  This field specifies the WLAN mode(s) supported by the target device. This is represented by a bit string, with a one value at the bit position means the WLAN mode is supported; a zero value means not supported. |
| ***wlan-MeasSupported***  This field specifies the measurements supported by the target device when accessing a WLAN. This is represented by a bit string, with a one‑value at the bit position means the particular measurement is supported; a zero‑value means not supported. A zero-value in all bit positions in the bit string means only the basic WLAN positioning method is supported by the target device which is reporting of the WLAN identity. The following bits are assigned for the indicated measurements.  rssi: AP signal strength at the target  rtt: Round Trip Time between target and AP |
| ***wlan-AP-AD-Supported*** This field specifies the WLAN AP assistance data supported by the target device. This is represented by a bit string, with a one-value at the bit position means the particular assistance data is supported; a zero-value means not supported. A zero-value in all bit positions or absence of this field means no assistance data is supported. The following bits are assigned for the indicated assistance data.  ap-identifier: WLAN AP identity information  ap-location: WLAN AP location information |
| ***periodicalReportingSupported***  This field, if present, specifies the positioning modes for which the target device supports *periodicalReporting*. This is represented by a bit string, with a one value at the bit position means *periodicalReporting* for the positioning mode is supported; a zero value means not supported. If this field is absent, the location server may assume that the target device does not support *periodicalReporting* in *CommonIEsRequestLocationInformation*. |
| ***idleStateForMeasurements***  This field, if present, indicates that the target device requires idle state to perform WLAN measurements. |
| ***scheduledLocationRequestSupported***  This field, if present, specifies the positioning modes for which the target device supports scheduled location requests – i.e., supports the IE *ScheduledLocationTime* in IE *CommonIEsRequestLocationInformation* – and the time base(s) supported for the scheduled location time for each positioning mode. If this field is absent, the target device does not support scheduled location requests. |
| ***periodicReportingIntervalMsSupport***  This field, if present, specified the supported minimum millisecond periodic reporting interval for location information per positioning mode – i.e., supports the subfield *reportingIntervalMs* of the IE *PeriodicalReportingCriteriaExt* in IE *CommonIEsRequestLocationInformation* – and the minimum millisecond report interval supported for the periodic reporting. |

#### 6.5.6.5 WLAN Capability Information Request

#### *–* *WLAN-RequestCapabilities*

The IE *WLAN-RequestCapabilities* is used by the location server to request WLAN positioning capabilities information from a target device.

-- ASN1START

WLAN-RequestCapabilities-r13 ::= SEQUENCE {

...

}

-- ASN1STOP

#### 6.5.6.6 WLAN Error Elements

#### *–* *WLAN-Error*

The IE *WLAN-Error* is used by the location server or target device to provide error reasons for WLAN positioning to the target device or location server, respectively.

-- ASN1START

WLAN-Error-r13 ::= CHOICE {

locationServerErrorCauses-r13 WLAN-LocationServerErrorCauses-r13,

targetDeviceErrorCauses-r13 WLAN-TargetDeviceErrorCauses-r13,

...

}

-- ASN1STOP

#### *–* *WLAN-LocationServerErrorCauses*

The IE *WLAN-LocationServerErrorCauses* is used by the location server to provide error reasons for WLAN positioning to the target device.

-- ASN1START

WLAN-LocationServerErrorCauses-r13 ::= SEQUENCE {

cause-r13 ENUMERATED {undefined,

...,

requestedADNotAvailable-v1420,

notAllrequestedADAvailable-v1420

},

...,

[[ apLocationDataUnavailable-r14 NULL OPTIONAL -- Need ON

]]

}

-- ASN1STOP

| ***WLAN-LocationServerErrorCauses* field descriptions** |
| --- |
| ***cause***  This field provides a WLAN AP specific error cause for the server applicable to provision of assistance data. If the cause value is '*requestedADNotAvailable*', none of the requested assistance data could be provided and no further information needs to be included. If the cause value is '*notAllRequestedADAvailable*', the server was able to provide some but not all requested WLAN AP assistance data. In this case, the server should include any of the specific error indications as applicable. Note that inclusion of these fields is applicable when some of the associated information can be provided for some WLAN APs but not for all WLAN APs. |

#### *–* *WLAN-TargetDeviceErrorCauses*

The IE *WLAN-TargetDeviceErrorCauses* is used by the target device to provide error reasons for WLAN positioning to the location server.

-- ASN1START

WLAN-TargetDeviceErrorCauses-r13 ::= SEQUENCE {

cause-r13 ENUMERATED {undefined,

requestedMeasurementsNotAvailable,

notAllrequestedMeasurementsPossible,

...

},

wlan-AP-RSSI-MeasurementNotPossible-r13 NULL OPTIONAL,

wlan-AP-RTT-MeasurementNotPossible-r13 NULL OPTIONAL,

...

}

-- ASN1STOP

| *WLAN-TargetDeviceErrorCauses* field descriptions |
| --- |
| ***cause***  This field provides a WLAN specific error cause. If the cause value is 'notAllRequestedMeasurementsPossible', the target device was not able to provide all requested WLAN measurements (but may be able to provide some measurements). In this case, the target device should include any of the *wlan‑AP‑RSSI‑MeasurementNotPossible*, or *wlan‑AP‑RTT‑MeasurementNotPossible* fields, as applicable. |

6.5.6.7 WLAN Assistance Data

*–* *WLAN-ProvideAssistanceData*

The IE *WLAN-ProvideAssistanceData* is used by the location server to provide assistance data to enable UE‑based and UE-assisted WLAN positioning. It may also be used to provide WLAN positioning specific error reason.

-- ASN1START

WLAN-ProvideAssistanceData-r14 ::= SEQUENCE {

wlan-DataSet-r14 SEQUENCE (SIZE (1..maxWLAN-DataSets-r14)) OF WLAN-DataSet-r14

OPTIONAL, -- Need ON

wlan-Error-r14 WLAN-Error-r13 OPTIONAL, -- Need ON

...

}

-- ASN1STOP

| ***WLAN-ProvideAssistanceData* field descriptions** |
| --- |
| ***wlan-DataSet*** This field provides data for sets of WLAN APs. |
| ***wlan-Error*** This field provides error information and may be included when a Provide Assistance Data is sent in response to a Request Assistance Data. It is allowed to include both a *wlan-DataSet* field and a *wlan-Error* field (e.g. when only some requested WLAN assistance data is provided). |

6.5.6.8 WLAN Assistance Data Elements

– *WLAN-DataSet*

The IE *WLAN-DataSet* is used by the location server to provide WLAN AP information for one set of WLAN APs.

-- ASN1START

WLAN-DataSet-r14 ::= SEQUENCE {

wlan-AP-List-r14 SEQUENCE (SIZE (1..maxWLAN-AP-r14)) OF WLAN-AP-Data-r14,

supportedChannels-11a-r14 SupportedChannels-11a-r14 OPTIONAL, -- Need ON

supportedChannels-11bg-r14 SupportedChannels-11bg-r14 OPTIONAL, -- Need ON

...

}

SupportedChannels-11a-r14 ::= SEQUENCE {

ch34-r14 BOOLEAN,

ch36-r14 BOOLEAN,

ch38-r14 BOOLEAN,

ch40-r14 BOOLEAN,

ch42-r14 BOOLEAN,

ch44-r14 BOOLEAN,

ch46-r14 BOOLEAN,

ch48-r14 BOOLEAN,

ch52-r14 BOOLEAN,

ch56-r14 BOOLEAN,

ch60-r14 BOOLEAN,

ch64-r14 BOOLEAN,

ch149-r14 BOOLEAN,

ch153-r14 BOOLEAN,

ch157-r14 BOOLEAN,

ch161-r14 BOOLEAN

}

SupportedChannels-11bg-r14 ::= SEQUENCE {

ch1-r14 BOOLEAN,

ch2-r14 BOOLEAN,

ch3-r14 BOOLEAN,

ch4-r14 BOOLEAN,

ch5-r14 BOOLEAN,

ch6-r14 BOOLEAN,

ch7-r14 BOOLEAN,

ch8-r14 BOOLEAN,

ch9-r14 BOOLEAN,

ch10-r14 BOOLEAN,

ch11-r14 BOOLEAN,

ch12-r14 BOOLEAN,

ch13-r14 BOOLEAN,

ch14-r14 BOOLEAN

}

-- ASN1STOP

| ***WLAN-DataSet* field descriptions** |
| --- |
| ***wlan-AP-List*** This field provides information for WLAN APs in the data set. |
| ***supportedChannels-11a*** This field defines the superset of all channels supported by all WLAN APs in the data set of type 801.11a (5GHz band). |
| ***supportedChannels-11bg*** This field defines the superset of all channels supported by all WLAN APs in the data set of type 801.11b or 802.11g (2.4 GHz band). |

– *WLAN-AP-Data*

The IE *WLAN-AP-Data* is used by the location server to provide information for one WLAN AP as part of WLAN AP assistance data.

-- ASN1START

WLAN-AP-Data-r14 ::= SEQUENCE {

wlan-AP-Identifier-r14 WLAN-AP-Identifier-r13,

wlan-AP-Location-r14 WLAN-AP-Location-r14 OPTIONAL, -- Need ON

...

}

WLAN-AP-Location-r14 ::= SEQUENCE {

locationDataLCI-r14 LocationDataLCI-r14,

...

}

LocationDataLCI-r14 ::= SEQUENCE {

latitudeUncertainty-r14 BIT STRING (SIZE (6)),

latitude-r14 BIT STRING (SIZE (34)),

longitudeUncertainty-r14 BIT STRING (SIZE (6)),

longitude-r14 BIT STRING (SIZE (34)),

altitudeUncertainty-r14 BIT STRING (SIZE (6)) OPTIONAL, -- Need ON

altitude-r14 BIT STRING (SIZE (30)) OPTIONAL, -- Need ON

datum-r14 BIT STRING (SIZE (8)),

...

}

-- ASN1STOP

| *WLAN-AP-Data* field descriptions |
| --- |
| ***wlan-AP-Location***  - ***locationDataLCI***  This field provides the location of the WLAN AP in the form of Location Configuration Information (LCI) defined in [27] and includes the following subfields:  latitudeUncertainty: 6-bits quantifying the amount of uncertainty in latitude. A value of 0 is reserved to indicate that the uncertainty is unknown; values greater than 34 are reserved. Its relation with the corresponding value in degrees is expressed with the following formula: latitudeUncertainty = 8 - ceil(log2(uncertainty in degrees))  latitude: A 34-bits fixed point value consisting of 9-bits of integer and 25-bits of fraction indicating the Latitude (+/- 90 degrees) of the AP.  longitudeUncertainty: 6-bits quantifying the amount of uncertainty in longitude. A value of 0 is reserved to indicate that the uncertainty is unknown; values greater than 34 are reserved. Its relation with the corresponding value in degrees is expressed with the following formula: longitudeUncertainty = 8 - ceil(log2(uncertainty in degrees))  longitude: A 34-bits fixed point value consisting of 9-bits of integer and 25-bits of fraction indicating the Longitude (+/- 180 degrees) of the AP.  altitudeUncertainty: 6-bits value quantifying the amount of uncertainty in the altitude value. A value of 0 is reserved to indicate that the uncertainty is unknown; values greater than 30 are reserved. Its relation with the corresponding value in metres is expressed with the following formula: altitudeUncertainty = 21 - ceil(log2( uncertainty in metres))  altitude: A 30-bit fixed point value consisting of 22-bits of integer and 8-bits of fraction indicating the altitude of the AP in metres.  datum: 8-bits indicating the map datum used for the coordinates. Defined codes are: Bit 1: World Geodetic System 1984 (WGS-84) Bit 2: North American Datum 1983 (NAD-83) with North American Vertical Datum 1988 (NAVD-88) Bit 3: North American Datum 1983 (NAD-83) with Mean Lower Low Water (MLLW) vertical datum.  Bits 4 – 8 are reserved. |

6.5.6.9 WLAN Assistance Data Request

*–* *WLAN-RequestAssistanceData*

The IE *WLAN-RequestAssistanceData* is used by the target device to request WLAN assistance data from a location server.

-- ASN1START

WLAN-RequestAssistanceData-r14 ::= SEQUENCE {

requestedAD-r14 BIT STRING { ap-identifier (0),

ap-location (1)} (SIZE (1..8)),

visibleAPs-r14 SEQUENCE (SIZE (1..maxVisibleAPs-r14)) OF WLAN-AP-Identifier-r13 OPTIONAL,

wlan-AP-StoredData-r14 SEQUENCE (SIZE (1..maxKnownAPs-r14)) OF WLAN-AP-Identifier-r13 OPTIONAL,

...

}

-- ASN1STOP

| ***WLAN-RequestAssistanceData* field descriptions** |
| --- |
| ***requestedAD*** This field specifies the WLAN AP assistance data requested. This is represented by a bit string, with a one-value at the bit position means the particular assistance data is requested; a zero-value means not requested. The following assistance data types are included:  ap-identifier: WLAN AP identity information ap-location: WLAN AP location information |
| ***visibleAPs*** This field enables a target to indicate to a server the identities of currently visible WLAN APs. This may assist a server to provide assistance data for WLAN APs nearby to the target. A target shall provide visible APs in order of received signal strength with the AP with the highest signal strength provided first. |
| ***wlan-AP-StoredData*** This field enables a target to indicate to a server the identities of WLAN APs for which the target has stored assistance data received previously from the server. This may enable the server to avoid resending data for the same APs. |

### 6.5.7 Bluetooth-based Positioning

#### 6.5.7.1 Bluetooth Location Information

#### *–* *BT-ProvideLocationInformation*

The IE *BT-ProvideLocationInformation* is used by the target device to provide measurements for one or more Bluetooth beacons to the location server. It may also be used to provide Bluetooth positioning specific error reason.

-- ASN1START

BT-ProvideLocationInformation-r13 ::= SEQUENCE {

bt-MeasurementInformation-r13 BT-MeasurementInformation-r13 OPTIONAL,

bt-Error-r13 BT-Error-r13 OPTIONAL,

...,

[[

bt-AoA-Config-r18 BT-AoA-Config-r18 OPTIONAL

]]

}

BT-AoA-Config-r18 ::= SEQUENCE {

bt-Addr-r18 BIT STRING (SIZE (48)),

cte-Status-r18 ENUMERATED { enabled } OPTIONAL,

primaryAdvInterval-r18 INTEGER (32..16777) OPTIONAL,

secondAdvInterval-r18 INTEGER (6..65535) OPTIONAL,

tx-Power-r18 INTEGER (-127..20) OPTIONAL,

cte-Length-r18 INTEGER (2..20) OPTIONAL,

cte-Count-r18 INTEGER (1..16) OPTIONAL,

tx-PHY-M2-r18 ENUMERATED { m2 } OPTIONAL,

...

}

-- ASN1STOP

| *BT-ProvideLocationInformation* field descriptions |
| --- |
| ***bt-Addr***  This field specifies the Bluetooth address of the device [53]. In case the device updates its address during an established LPP session, the device shall provide the new address as unsolicited location information to the server. |
| ***cte-Status***  This field provides the Bluetooth AoA transmission status of the device: If the field is present and set to *enabled*, the Bluetooth AoA transmission is enabled and if the field is not present, the Bluetooth AoA transmission is *disabled*. |
| ***primaryAdvInterval***  This field specifies the Bluetooth primary advertisement channel periodicity that the device will use. Scaling factor 0.625 ms [53]. |
| ***secondAdvInterval***  This field specifies the Bluetooth periodic advertising interval on secondary advertisement channels that the device will use. Scaling factor 0.625 ms [53]. |
| ***tx-Power***  This field specifies the Bluetooth advertising TX power in dBm that the device will use. |
| ***cte-Length***  This field specifies the configured CTE length to be used by the device in number of 8 µs segments. |
| ***cte-Count***  This field specifies the number of Bluetooth packets that include a CTE that the device will transmit each periodic advertising. |
| ***tx-PHY-M2***  This field, if present, indicates that Bluetooth TX PHY 2 Megasymbols/s will be used for AoA, otherwise Bluetooth TX PHY 1 Megasymbols/s will be used. |

#### 6.5.7.2 Bluetooth Location Information Elements

#### *–* *BT-MeasurementInformation*

-- ASN1START

BT-MeasurementInformation-r13 ::= SEQUENCE {

measurementReferenceTime-r13 UTCTime OPTIONAL,

bt-MeasurementList-r13 BT-MeasurementList-r13 OPTIONAL,

...,

[[

bt-MeasurementList-r18 BT-MeasurementList-r18 OPTIONAL

]]

}

BT-MeasurementList-r13 ::= SEQUENCE (SIZE(1..maxBT-Beacon-r13)) OF BT-MeasurementElement-r13

BT-MeasurementElement-r13 ::= SEQUENCE {

btAddr-r13 BIT STRING (SIZE (48)),

rssi-r13 INTEGER (-128..127) OPTIONAL,

...

}

BT-MeasurementList-r18 ::= SEQUENCE (SIZE(1..maxBT-Beacon-r13)) OF BT-MeasurementElement-r18

BT-MeasurementElement-r18 ::= SEQUENCE {

btAddr-r18 BIT STRING (SIZE (48)),

bt-azimuth-r18 INTEGER (0..359),

bt-elevation-r18 INTEGER (0..180) OPTIONAL,

rssi-r18 INTEGER (-128..127) OPTIONAL,

...

}

-- ASN1STOP

| *BT-MeasurementInformation* field descriptions |
| --- |
| ***measurementReferenceTime***  This field provides the UTC time when the Bluetooth measurements are performed and should take the form of *YYMMDDhhmmssZ*. |
| ***bt-MeasurementList***  This field provides the Bluetooth measurements for up to 32 Bluetooth beacons. |
| ***btAddr***  This field specifies the Bluetooth public address of the Bluetooth beacon [25]. |
| ***rssi***  This field provides the beacon received signal strength indicator (RSSI) in dBm. |
| ***bt-azimuth***  This field represents the estimated AoD azimuth in GCD relative the Bluetooth beacon reference position. |
| ***bt-elevation***  This field represents the estimated AoD elevation in GCD relative the Bluetooth beacon reference position. |

#### 6.5.7.3 Bluetooth Location Information Request

#### *–* *BT-RequestLocationInformation*

The IE *BT-RequestLocationInformation* is used by the location server to request Bluetooth measurements from a target device.

-- ASN1START

BT-RequestLocationInformation-r13 ::= SEQUENCE {

requestedMeasurements-r13 BIT STRING {

rssi (0),

aod-v1800 (1)} (SIZE(1..8)),

...,

[[

bt-requestedAoA-Config-r18 BIT STRING {

aoa-advConfig (0),

aoa-cteConfig (1)} (SIZE(1..8)) OPTIONAL, -- Need ON

bt-suggestedAoA-Config-r18 BT-SuggestedAoA-Config-r18 OPTIONAL -- Need ON

]]

}

BT-SuggestedAoA-Config-r18 ::= SEQUENCE {

cte-Status-r18 ENUMERATED {enabled, disabled} OPTIONAL, -- Need ON

primaryAdvInterval-r18 INTEGER (32..16777) OPTIONAL, -- Need ON

secondAdvInterval-r18 INTEGER (6..65535) OPTIONAL, -- Need ON

tx-Power-r18 INTEGER (-127..20) OPTIONAL, -- Need ON

cte-Length-r18 INTEGER (2..20) OPTIONAL, -- Need ON

cte-Count-r18 INTEGER (1..16) OPTIONAL, -- Need ON

tx-PHY-M2-r18 ENUMERATED { m2 } OPTIONAL, -- Need OP

...

}

-- ASN1STOP

| *BT-RequestLocationInformation* field descriptions |
| --- |
| ***requestedMeasurements***  This field specifies the Bluetooth measurements requested. This is represented by a bit string, with a one‑value at the bit position means the particular measurement is requested; a zero‑value means not requested. The following measurement requests can be included:  rssi: Bluetooth beacon signal strength at the target.  aod: Estimated AoD per Bluetooth beacon. |
| ***bt-requestedAoA-Config***  This field specifies the Bluetooth AoA configuration parameters requested. This is represented by a bit string, with a one‑value at the bit position means the particular measurement is requested; a zero‑value means not requested. The following information requests can be included:  aoa-advConfig: The Bluetooth advertisement address and periodic intervals of the device.  aoa-cteConfig: The configured CTE status, length, count and PHY. |
| ***cte-Status***  This field suggests the Bluetooth AoA transmission status of the device, and is used by the location server to suggest BLE AoA transmission of the device to be enabled or disabled:  enabled: Bluetooth AoA transmission is suggested enabled.  disabled: Bluetooth AoA transmission is suggested disabled. |
| ***primaryAdvInterval***  This field suggests the Bluetooth primary advertisement channel periodicity of the device, scaling factor 0.625 ms [53]. |
| ***secondAdvInterval***  This field suggests the Bluetooth periodic advertising interval on secondary advertisement channels of the device, scaling factor 0.625 ms [53]. |
| ***tx-Power***  This field suggests the Bluetooth advertising TX power in dBm of the device [53]. |
| ***cte-Length***  This field suggests the CTE length of the device in number of 8 µs segments. |
| ***cte-Count***  This field suggests the number of Bluetooth packets that include a CTE of the device each periodic advertising event. |
| ***tx-PHY-M2***  This field, if present, suggests that Bluetooth TX PHY 2 Megasymbols/s is used for AoA, otherwise Bluetooth TX PHY 1 Megasymbols/s is suggested to be used by the device. |

#### 6.5.7.4 Bluetooth Capability Information

#### *–* *BT-ProvideCapabilities*

The IE *BT-ProvideCapabilites* is used by the target device to provide its capabilities for Bluetooth positioning to the location server.

-- ASN1START

BT-ProvideCapabilities-r13 ::= SEQUENCE {

bt-Modes-r13 BIT STRING { standalone (0),

ue-assisted (1),

ue-based-v1810 (2)} (SIZE (1..8)),

bt-MeasSupported-r13 BIT STRING { rssi-r13 (0),

aod-v1800 (1)} (SIZE (1..8)),

...,

[[

idleStateForMeasurements-r14

ENUMERATED { required } OPTIONAL,

periodicalReportingSupported-r14

PositioningModes OPTIONAL

]],

[[ scheduledLocationRequestSupported-r17 ScheduledLocationTimeSupportPerMode-r17 OPTIONAL

]],

[[ bt-AoA-r18 ENUMERATED { request-only, suggestion } OPTIONAL,

periodicReportingIntervalMsSupport-r18 PeriodicReportingIntervalMsSupportPerMode-r18

OPTIONAL

]]

}

-- ASN1STOP

| *BT-ProvideCapabilities* field descriptions |
| --- |
| ***bt-Modes***  This field specifies the Bluetooth mode(s) supported by the target device. This is represented by a bit string, with a one value at the bit position means the Bluetooth mode is supported; a zero value means not supported. |
| ***bt-MeasSupported***  This field specifies the Bluetooth measurements supported by the target device. This is represented by a bit string, with a one‑value at the bit position means the particular measurement is supported; a zero‑value means not supported. A zero-value in all bit positions in the bit string means only the basic Bluetooth positioning method is supported by the target device which is reporting of the Bluetooth beacon identity. The following bits are assigned for the indicated measurements.  - rssi: Bluetooth beacon signal strength at the target device.  - aod: Bluetooth beacon AoD at the target device. |
| ***idleStateForMeasurements***  This field, if present, indicates that the target device requires idle state to perform BT measurements. |
| ***periodicalReportingSupported***  This field, if present, specifies the positioning modes for which the target device supports *periodicalReporting*. This is represented by a bit string, with a one value at the bit position means *periodicalReporting* for the positioning mode is supported; a zero value means not supported. If this field is absent, the location server may assume that the target device does not support *periodicalReporting* in *CommonIEsRequestLocationInformation*. |
| ***scheduledLocationRequestSupported***  This field, if present, specifies the positioning modes for which the target device supports scheduled location requests – i.e., supports the IE *ScheduledLocationTime* in IE *CommonIEsRequestLocationInformation* – and the time base(s) supported for the scheduled location time for each positioning mode. If this field is absent, the target device does not support scheduled location requests. |
| ***bt-AoA***  This field, if present, indicates that the target device supports Bluetooth AoA, where:  - request-only: Target device supports to provide its Bluetooth AoA transmission configuration to LMF upon request.  - suggestion: Target device supports obtaining a suggestion from LMF about device Bluetooth AoA transmission configuration and device supports to provide its Bluetooth AoA transmission configuration based on the suggestion back to LMF. |
| ***periodicReportingIntervalMsSupport***  This field, if present, specified the supported minimum millisecond periodic reporting interval for location information per positioning mode – i.e., supports the subfield *reportingIntervalMs* of the IE *PeriodicalReportingCriteriaExt* in IE *CommonIEsRequestLocationInformation* – and the minimum millisecond report interval supported for the periodic reporting. |

#### 6.5.7.5 Bluetooth Capability Information Request

#### *–* *BT-RequestCapabilities*

The IE *BT-RequestCapabilities* is used by the location server to request Bluetooth positioning capabilities from a target device.

-- ASN1START

BT-RequestCapabilities-r13 ::= SEQUENCE {

...

}

-- ASN1STOP

#### 6.5.7.6 BT Error Elements

#### *–* *BT-Error*

The IE *BT-Error* is used by the location server or target device to provide error reasons for Bluetooth positioning to the target device or location server, respectively.

-- ASN1START

BT-Error-r13 ::= CHOICE {

locationServerErrorCauses-r13 BT-LocationServerErrorCauses-r13,

targetDeviceErrorCauses-r13 BT-TargetDeviceErrorCauses-r13,

...

}

-- ASN1STOP

#### *–* *BT-LocationServerErrorCauses*

The IE *BT-LocationServerErrorCauses* is used by the location server to provide error reasons for Bluetooth positioning to the target device.

-- ASN1START

BT-LocationServerErrorCauses-r13 ::= SEQUENCE {

cause-r13 ENUMERATED {undefined, ...,

assistanceDataNotSupportedByServer-v1810,

assistanceDataSupportedButCurrentlyNotAvailableByServer-v1810,

notAllrequestedAssistanceDataAvailableByServer-v1810

},

...

}

-- ASN1STOP

#### – *BT-TargetDeviceErrorCauses*

The IE *BT-TargetDeviceErrorCauses* is used by the target device to provide error reasons for Bluetooth positioning to the location server.

-- ASN1START

BT-TargetDeviceErrorCauses-r13 ::= SEQUENCE {

cause-r13 ENUMERATED {undefined,

requestedMeasurementsNotAvailable,

notAllrequestedMeasurementsPossible,

...,

assistanceDataMissing-v1810

},

bt-Beacon-rssiMeasurementNotPossible-r13 NULL OPTIONAL,

...

}

-- ASN1STOP

| *BT-TargetDeviceErrorCauses* field descriptions |
| --- |
| ***cause***  This field provides a Bluetooth specific error cause. If the cause value is 'notAllRequestedMeasurementsPossible', the target device was not able to provide all requested Bluetooth measurements (but may be able to provide some measurements). In this case, the target device should include *bt-Beacon-rssiMeasurementNotPossible* field. |

#### 6.5.7.7 Bluetooth Assistance Data

#### – *BT-ProvideAssistanceData*

The IE *BT-ProvideAssistanceData* is used by the location server to provide assistance data to enable UE‑based and UE-assisted AoD positioning. It may also be used to provide Bluetooth positioning specific error reasons.

-- ASN1START

BT-ProvideAssistanceData-r18 ::= SEQUENCE {

bt-BeaconInfo-r18 BT-BeaconInfo-r18,

bt-Error-r18 BT-Error-r13 OPTIONAL, -- Need ON

...

}

-- ASN1STOP

| *BT-ProvideAssistanceData* field descriptions |
| --- |
| ***bt-BeaconInfo*** This field provides data for a set of Bluetooth beacons. |
| ***bt-Error*** This field provides error information and may be included when a Provide Assistance Data is sent in response to a Request Assistance Data. |

#### 6.5.7.8 Bluetooth Assistance Data Elements

#### – *BT-BeaconInfo*

The IE *BT-BeaconInfo* is used by the location server to provide Bluetooth beacon information for one set of Bluetooth beacons.

-- ASN1START

BT-BeaconInfo-r18 ::= SEQUENCE {

referencePoint-r18 ReferencePoint-r16,

bt-BeaconInfoList-r18 SEQUENCE (SIZE (1..maxBT-BeaconAD-r18)) OF

BT-BeaconInfoElement-r18,

...

}

BT-BeaconInfoElement-r18 ::= SEQUENCE {

bt-Addr-r18 BIT STRING (SIZE (48)),

bt-BeaconLocation-r18 RelativeLocation-r16 OPTIONAL, -- Need OP

bt-LCS-GCS-TranslationParameter-r18 LCS-GCS-TranslationParameter-r16

OPTIONAL, -- Cond NotSameAsPrev1

bt-antArrayConfig-r18 BT-AntArrayConfig-r18 OPTIONAL, -- Cond NotSameAsPrev2

bt-antElementList-r18 SEQUENCE (SIZE (2..maxBT-BeaconAntElt-r18)) OF

BT-AntElement-r18 OPTIONAL, -- Cond NotSameAsPrev3

bt-antSwitchingPattern-r18 SEQUENCE (SIZE (2..maxBT-BeaconAntElt-r18)) OF

BT-AntSwitchElement-r18 OPTIONAL, -- Cond NotSameAsPrev4

bt-AoD-TransmConfig-r18 BT-AoD-TransmConfig-r18 OPTIONAL, -- Cond NotSameAsPrev5

...

}

BT-AntArrayConfig-r18 ::= CHOICE {

bt-UniformLinearArray-r18 BT-UniformLinearArray-r18,

bt-UniformRectangularArray-r18 BT-UniformRectangularArray-r18,

bt-UniformCircularArray-r18 BT-UniformCircularArray-r18,

bt-GenericArray-r18 BT-GenericArray-r18

}

BT-AntElement-r18 ::= SEQUENCE {

polarization-r18 ENUMERATED {m45, zero, p45, p90, circ},

...

}

BT-AntSwitchElement-r18 ::= SEQUENCE {

antElementIndexShort-r18 INTEGER (1..16),

antElementIndexOffset-r18 ENUMERATED {o16, o32, o48, o64} OPTIONAL, -- Need OP

...

}

BT-AoD-TransmConfig-r18 ::= SEQUENCE {

primaryAdvInterval-r18 INTEGER (32..16777),

secondAdvInterval-r18 INTEGER (6..65535),

cte-Length-r18 INTEGER (2..20),

cte-Count-r18 INTEGER (1..16),

cte-Type2us-r18 ENUMERATED { true } OPTIONAL, -- Need OP

tx-PHY-M2-r18 ENUMERATED { true } OPTIONAL, -- Need OP

...

}

-- ASN1STOP

| Conditional presence | Explanation |
| --- | --- |
| *NotSameAsPrev1* | The field is mandatory present in the first element of the *bt-BeaconInfoList* list; otherwise if not present, the *bt-LCS-GCS-TranslationParameter* of this element is the same as the *bt-LCS-GCS-TranslationParameter* of theprevious element in the *bt-BeaconInfoList* list. |
| *NotSameAsPrev2* | The field is mandatory present in the first element of the *bt-BeaconInfoList* list; otherwise if not present, the *bt-antArrayConfig* of this element is the same as the *bt-antArrayConfig* of theprevious element in the *bt-BeaconInfoList* list. |
| *NotSameAsPrev3* | The field is mandatory present in the first element of the *bt-BeaconInfoList* list; otherwise if not present, the *bt-antElementList* of this element is the same as the *bt-antElementList* of theprevious element in the *bt-BeaconInfoList* list. |
| *NotSameAsPrev4* | The field is mandatory present in the first element of the *bt-BeaconInfoList* list; otherwise if not present, the *bt-antSwitchingPattern* of this element is the same as the *bt-antSwitchingPattern* of theprevious element in the *bt-BeaconInfoList* list. |
| *NotSameAsPrev5* | The field is mandatory present in the first element of the *bt-BeaconInfoList* list; otherwise if not present, the *bt-AoDTransmConfig* of this element is the same as the *bt-AoDTransmConfig* of theprevious element in the *bt-BeaconInfoList* list. |

| *BT-BeaconInfo* field descriptions |
| --- |
| ***bt-Addr***  This field specifies the Bluetooth public address of the Bluetooth beacon [53]. |
| ***referencePoint***  This field specifies the reference point used to define the locations of the set of Bluetooth beacons. |
| ***bt-BeaconLocation***  This field provides the location of the Bluetooth beacon relative to the *referencePoint* location. If this field is absent the Bluetooth beacon location coincides with the *referencePoint* location. |
| ***bt-LCS-GCS-TranslationParameter***  This field provides the angles α (bearing angle), β (downtilt angle) and γ (slant angle) for the translation of a Local Coordinate System (LCS) to a Global Coordinate System (GCS) as defined in TR 38.901 [44]. |
| ***polarization***  This field specifies the antenna element polarization in degrees relative the positive y-axis, where *m45*, *zero*, *p45*, *p90* represents -45, zero, 45 and 90 degrees respectively towards the z-axis, and *circ* represents circular polarization. |
| ***bt-AoD-TransmConfig***  This field specifies Bluetooth beacon AoD transmission configuration in terms of advertising periodicities and CTE configuration to support the device to configure its scan windows and intervals. |
| ***primaryAdvInterval***  This field specifies the Bluetooth primary advertisement channel periodicity used by the Bluetooth beacon, scaling factor 0.625 ms [53]. |
| ***secondAdvInterval***  This field specifies the Bluetooth periodic advertising interval on secondary advertisement channels used by the Bluetooth beacon, scaling factor 0.625 ms [53]. |
| ***cte-Length***  This field specifies the configured CTE length to be used by the beacon in number of 8 µs segments. |
| ***cte-Count***  This field specifies the number of Bluetooth packets that include a CTE that are transmitted each periodic advertising event. |
| ***cte-Type2us***  This field, if present, indicates that 2 µs antenna switching slot duration is used by the beacon, otherwise 1 µs antenna switching slot duration is used. |
| ***tx-PHY-M2***  This field, if present, indicates that Bluetooth TX PHY 2 Megasymbols/s is used by the beacon, otherwise Bluetooth TX PHY 1 Megasymbols/s is used. |
| ***bt-antSwitchingPattern***  This field specifies the Bluetooth antenna switching pattern as a list of indices, where each index is the order value of a specific antenna element in the *bt-antElementList-r18* attribute of the IE *BT-BeaconInfoElement-r18* – first element in the list corresponds to index 1 and so on. If the antenna switching pattern is shorter than the number of available sample slots, then the antenna switching patterns continues from the beginning of the *bt-antSwitchingPattern-r18*. If antenna switching pattern is longer than the number of available sample slots, then the elements in *bt-antSwitchingPattern-r18* are discarded. If this field is not present, the target device can assume an antenna switching pattern with the configured antenna element in the same order as in the *bt-antElementList-r18*. |
| ***antElementIndexShort***  This field specifies short part of the antenna element index. |
| ***antElementIndexOffset***  This field specifies offset of the antenna element index, where o16, o32, o48 and o64 respresents 16, 32, 48 and 64 respectively to offset the short part of the antenna element index. If not present, the offset is zero. |

#### *–* *BT-UniformLinearArray*

The IE *BT-UniformLinearArray* is used by the location server to define a linear antenna array as a formula based on the antenna element index.

-- ASN1START

BT-UniformLinearArray-r18 ::= SEQUENCE {

bt-NoElements-r18 INTEGER (2..maxBT-BeaconAntElt-r18),

bt-InterElementDist-r18 INTEGER (30..130)

}

-- ASN1STOP

| *BT-UniformLinearArray* field descriptions |
| --- |
| ***bt-NoElements***  This field specifies the number of antenna elements in the linear antenna array. It is the same as the number of antenna elements in the *bt-antElementList-r18* of the IE *BT-BeaconInfoElement-r18*. |
| ***bt-InterElementDist***  This field specifies the distance between to adjacent elements in the uniform linear antenna array between ¼ and just above 1 wavelength. Scale factor 1mm. |

The antenna element locations of the antenna array are defined along the y-axis from the reference point. The coordinates of the elements are *x=0, z=0* and *y = (index-1)\*bt-InterElementDist-r18*, where *index* is the order value of a specific antenna element in the *bt-antElementList-r18* attribute of the IE *BT-BeaconInfoElement-r18* – first element in the list corresponds to index 1 and so on.

#### *– BT-UniformRectangularArray*

The IE *BT-UniformRectangularArray* is used by the location server to define a rectangular antenna array as a formula based on the antenna element index.

-- ASN1START

BT-UniformRectangularArray-r18 ::= SEQUENCE {

bt-NoElementsY-r18 INTEGER (1..maxBT-BeaconAntElt-r18),

bt-NoElementsZ-r18 INTEGER (1..maxBT-BeaconAntElt-r18),

bt-InterElementDistY-r18 INTEGER (30..135),

bt-InterElementDistZ-r18 INTEGER (30..135)

}

-- ASN1STOP

| *BT-UniformRectangularArray* field descriptions |
| --- |
| ***bt-NoElementsY***  This field specifies the number of antenna elements in the L-shaped antenna array along the y-axis. The product *bt-ElementDeltaY*\* *bt-ElementDeltaZ* is the same as the number of antenna elements in the *bt-antElementList-r18* of the IE *BT-BeaconInfoElement-r18*. |
| ***bt-NoElementsZ***  This field specifies the number of antenna elements in the linear antenna array along the z-axis. |
| ***bt-InterElementDistY***  This field specifies the distance between to adjacent elements in the uniform rectangular antenna array along the y-axis. |
| ***bt-InterElementDistZ***  This field specifies the distance between to adjacent elements in the uniform rectangular antenna array along the z-axis. |

The antenna element locations of the uniform rectangular antenna array are defined row by row along the y-axis with an increasing offset in the z-direction for each row from the reference point. The coordinates of the elements of the

- first row are x=*0*, z=*0* and *y* = (*index-1*)\**bt-InterElementDistY-r18*, for index 1 to *bt-NoElementsY*

- second row are x=*0*, *z* = *bt-InterElementDistZ* and *y* = (*index-bt-NoElementsY*-*1*)\**bt-InterElementDistY-r18*, for index (*bt-NoElementsY*+*1*) to *2*\**bt-NoElementsY*

- row *N* are x=*0*, *z* = (*N-1*)\**bt-InterElementDistZ* and *y* = (*index*-(*N-1*)\**bt-NoElementsY-1*)\**bt-InterElementDistY-r18*, for index ((*N-1*)\**bt-NoElementsY+1*) to *N*\**bt-NoElementsY*, where N = *1* to *bt-NoElementsZ*.

#### *– BT-UniformCircularArray*

The IE *BT-UniformCircularArray* is used by the location server to define a uniform circular antenna array as a formula based on the antenna element index.

-- ASN1START

BT-UniformCircularArray-r18 ::= SEQUENCE {

bt-NoElements-r18 INTEGER (2..maxBT-BeaconAntElt-r18),

bt-InterElementDist-r18 INTEGER (30..130)

}

-- ASN1STOP

| *BT-UniformCircularArray* field descriptions |
| --- |
| ***bt-NoElements***  This field specifies the number of antenna elements in the circular antenna array. It is the same as the number of antenna elements in the *bt-antElementList-r18* of the IE *BT-BeaconInfoElement-r18* |
| ***bt-InterElementDist***  This field specifies the distance between to adjacent elements in the uniform circular antenna array between ¼ and just above 1 wavelengths. Scale factor 1mm. |

The antenna element locations of the antenna array are defined along a circle with the reference point as center. The coordinates of the elements are:

- *x*=*0*

- *y* = *bt-Radius*\* cos(*2\*p*\*(*index-1*)/ *bt-NoElements-r18*)

- *z* = *bt-Radius*\* sin(*2\*p*\*(*index-1*)/ *bt-NoElements-r18*)

where *index* is the order value of a specific antenna element in the *bt-antElementList-r18* attribute of the IE *BT-BeaconInfoElement-r18* – first element in the list corresponds to index 1 and so on, and

*bt-Radius* = *bt-InterElementDist-r18*/(2\*sin(p / *bt-NoElements-r18*))

#### *– BT-GenericArray*

The IE *BT-GenericArray* is used by the location server to define a generic antenna array as a list of offset locations for each antenna element, where each ordered entry in *BT-GenericArray-r18* is associated to the same ordered entry in the *bt-antElementList-r18* attribute of the IE *BT-BeaconInfoElement-r18.*

-- ASN1START

BT-GenericArray-r18 ::= SEQUENCE (SIZE (2..maxBT-BeaconAntElt-r18)) OF BT-ULA-GenericAntElement-r18

BT-ULA-GenericAntElement-r18 ::= SEQUENCE {

deltaY-r18 INTEGER (-135..135) OPTIONAL, -- Need OP

deltaX-r18 INTEGER (-135..135) OPTIONAL, -- Need OP

deltaZ-r18 INTEGER (-135..135) OPTIONAL -- Need OP

}

-- ASN1STOP

| *BT-GenericArray* field descriptions |
| --- |
| ***deltaX, deltaY, deltaZ***  This field specifies the antenna element location offset in X, Y, Z directions respectively. If not present, the delta is zero. Scale factor 1mm. |

#### 6.5.7.9 Bluetooth Assistance Data Request

#### *– BT-RequestAssistanceData*

The IE *BT-RequestAssistanceData* is used by the target device to request BT assistance data from a location server.

-- ASN1START

BT-RequestAssistanceData-r18 ::= SEQUENCE {

requestedAD-r18 BIT STRING {

beacon-location (0),

beacon-antConfig (1),

beacon-transmConfig (2) } (SIZE (1..8)),

...

}

-- ASN1STOP

| *BT-RequestAssistanceData* field descriptions |
| --- |
| ***requestedAD*** This field specifies the Bluetooth assistance data requested. This is represented by a bit string, with a one-value at the bit position means the particular assistance data is requested; a zero-value means not requested. The following assistance data types are included:  *-* *beacon-location*: Bluetooth beacon location information  *-* *beacon-antConfig*: Bluetooth beacon antenna orientation, array configuration information and antenna switching pattern for AoD estimation  - *beacon-transmConfig*: Bluetooth beacon advertisement and CTE configuration information |

### 6.5.8 NR UL Positioning

#### 6.5.8.1 NR UL Capability Information

#### *– NR-UL-ProvideCapabilities*

The IE *NR-UL-ProvideCapabilities* is used by the target device to indicate its capability to support UL SRS for positioning and to provide its UL SRS for positioning capabilities to the location server.

-- ASN1START

NR-UL-ProvideCapabilities-r16 ::= SEQUENCE {

nr-UL-SRS-Capability-r16 NR-UL-SRS-Capability-r16,

...,

[[

nr-UE-TEG-Capability-r17 NR-UE-TEG-Capability-r17 OPTIONAL

]]

}

-- ASN1STOP

| *NR-UL-ProvideCapabilities* field descriptions |
| --- |
| ***nr-UE-TEG-Capability***  Indicates the UE TEG capability. |

#### 6.5.8.2 NR UL Capability Information Request

#### *– NR-UL-RequestCapabilities*

The IE *NR-UL-RequestCapabilities* is used by the location server to request the capability of the target device to support UL SRS for positioning and to request UL SRS for positioning capabilities from a target device.

-- ASN1START

NR-UL-RequestCapabilities-r16 ::= SEQUENCE {

...

}

-- ASN1STOP

### 6.5.9 NR E-CID Positioning

This clause defines the information elements for NR E-CID positioning (TS 38.305 [40]).

#### 6.5.9.1 NR E-CID Location Information

#### – *NR-ECID-ProvideLocationInformation*

The IE *NR-ECID-ProvideLocationInformation* is used by the target device to provide NR E-CID location measurements to the location server. It may also be used to provide NR E-CID positioning specific error reason.

-- ASN1START

NR-ECID-ProvideLocationInformation-r16 ::= SEQUENCE {

nr-ECID-SignalMeasurementInformation-r16 NR-ECID-SignalMeasurementInformation-r16 OPTIONAL,

nr-ECID-Error-r16 NR-ECID-Error-r16 OPTIONAL,

...

}

-- ASN1STOP

#### 6.5.9.2 NR E-CID Location Information Elements

#### – *NR-ECID-SignalMeasurementInformation*

The IE *NR-ECID-SignalMeasurementInformation* is used by the target device to provide NR E-CID measurements to the location server.

-- ASN1START

NR-ECID-SignalMeasurementInformation-r16 ::= SEQUENCE {

nr-PrimaryCellMeasuredResults-r16 NR-MeasuredResultsElement-r16,

nr-MeasuredResultsList-r16 NR-MeasuredResultsList-r16 OPTIONAL,

...

}

NR-MeasuredResultsList-r16 ::= SEQUENCE (SIZE(1..32)) OF NR-MeasuredResultsElement-r16

NR-MeasuredResultsElement-r16 ::= SEQUENCE {

nr-PhysCellID-r16 NR-PhysCellID-r16,

nr-ARFCN-r16 CHOICE {

ssb-ARFCN-r16 ARFCN-ValueNR-r15,

csi-RS-pointA-r16 ARFCN-ValueNR-r15

},

nr-CellGlobalID-r16 NCGI-r15 OPTIONAL,

systemFrameNumber-r16 BIT STRING (SIZE (10)) OPTIONAL, resultsSSB-Cell-r16 MeasQuantityResults-r16 OPTIONAL,

resultsCSI-RS-Cell-r16 MeasQuantityResults-r16 OPTIONAL,

resultsSSB-Indexes-r16 ResultsPerSSB-IndexList-r16 OPTIONAL,

resultsCSI-RS-Indexes-r16 ResultsPerCSI-RS-IndexList-r16 OPTIONAL,

...

}

MeasQuantityResults-r16 ::= SEQUENCE {

nr-RSRP-r16 INTEGER (0..127) OPTIONAL,

nr-RSRQ-r16 INTEGER (0..127) OPTIONAL

}

ResultsPerSSB-IndexList-r16::= SEQUENCE (SIZE (1..64)) OF ResultsPerSSB-Index-r16

ResultsPerSSB-Index-r16 ::= SEQUENCE {

ssb-Index-r16 INTEGER (0..63),

ssb-Results-r16 MeasQuantityResults-r16

}

ResultsPerCSI-RS-IndexList-r16::= SEQUENCE (SIZE (1..64)) OF ResultsPerCSI-RS-Index-r16

ResultsPerCSI-RS-Index-r16 ::= SEQUENCE {

csi-RS-Index-r16 INTEGER (0..95),

csi-RS-Results-r16 MeasQuantityResults-r16

}

-- ASN1STOP

| *NR-ECID-SignalMeasurementInformation* field descriptions |
| --- |
| ***nr-PrimaryCellMeasuredResults***  This field contains the NR E-CID measurements for the primary cell. |
| ***nr-MeasuredResultsList***  This field contains the NR E-CID measurements for up to 32 neighbour cells. |
| ***nr-PhysCellID***  This field specifies the NR physical cell identity of the measured cell. |
| ***nr-ARFCN***  This field specifies the ARFCN of the first RE of SSB's RB#10 or the point A of CSI-RS. |
| ***nr-CellGlobalID***  This field specifies the NR cell global ID of the measured cell. The target device shall provide this field if it was able to determine the NCGI of the measured cell at the time of measurement. |
| ***systemFrameNumber***  This field specifies the system frame number of the measured cell during which the measurements have been performed. The target device shall include this field if it was able to determine the SFN of the cell at the time of measurement. |
| ***resultsSSB-Cell***  This field specifies the SS reference signal received power (SS-RSRP) and quality (SS-RSRQ) measurement aggregated at cell level, as defined in TS 38.331 [35]. |
| ***resultsCSI-RS-Cell***  This field specifies the CSI-RS reference signal received power (CSI-RSRP) and quality (CSI-RSRQ) measurement aggregated at cell level, as defined in TS 38.331 [35]. |
| ***resultsSSB-Indexes***  This field specifies the SS reference signal received power (SS-RSRP) and quality (SS-RSRQ) measurement per SSB resource, as defined in TS 38.331 [35]. |
| ***resultsCSI-RS-Indexes***  This field specifies the CSI-RS reference signal received power (CSI-RSRP) and quality (CSI-RSRQ) per CSI-RS resource, as defined in TS 38.331 [35]. |
| ***nr-RSRP***  This field specifies the integer value for RSRP measurements according to Table 10.1.6.1-1 in TS 38.133 [46]. |
| ***nr-RSRQ***  This field specifies the integer value for RSRQ measurements accordng to Table 10.1.11.1-1 in TS 38.133 [46]. |

#### 6.5.9.3 NR E-CID Location Information Request

#### – *NR-ECID-RequestLocationInformation*

The IE *NR-ECID-RequestLocationInformation* is used by the location server to request NR E-CID location measurements from a target device.

-- ASN1START

NR-ECID-RequestLocationInformation-r16 ::= SEQUENCE {

requestedMeasurements-r16 BIT STRING { ssrsrpReq (0),

ssrsrqReq (1),

csirsrpReq (2),

csirsrqReq (3)} (SIZE(1..8)),

...

}

-- ASN1STOP

| *NR-ECID-RequestLocationInformation* field descriptions |
| --- |
| ***requestedMeasurements***  This field specifies the NR E-CID measurements requested. This is represented by a bit string, with a one‑value at the bit position means the particular measurement is requested; a zero‑value means not requested. |

#### 6.5.9.4 NR E-CID Capability Information

#### – *NR-ECID-ProvideCapabilities*

The IE *NR-ECID-ProvideCapabilities* is used by the target device to indicate its capability to support NR E-CID and to provide its NR E-CID positioning capabilities to the location server.

-- ASN1START

NR-ECID-ProvideCapabilities-r16 ::= SEQUENCE {

nr-ECID-MeasSupported-r16 BIT STRING { ssrsrpSup (0),

ssrsrqSup (1),

csirsrpSup (2),

csirsrqSup (3)} (SIZE(1..8)),

periodicalReporting-r16 ENUMERATED { supported } OPTIONAL,

triggeredReporting-r16 ENUMERATED { supported } OPTIONAL,

...,

[[

ten-ms-unit-ResponseTime-r17 ENUMERATED { supported } OPTIONAL,

scheduledLocationRequestSupported-r17

ScheduledLocationTimeSupport-r17 OPTIONAL

]],

[[ periodicReportingIntervalMsSupport-r18 PeriodicReportingIntervalMsSupport-r18 OPTIONAL

]]

}

-- ASN1STOP

| *NR-ECID-ProvideCapabilities* field descriptions |
| --- |
| ***nr-ECID-MeasSupported:***  Indicates the supported NR ECID measurements:  - *ssrsrpSup* indicates the UE supports SSB based cell/beam specific RSRP measurement;  - *ssrsrqSup* indicates the UE supports SSB based cell/beam specific RSRQ measurement;  - *csirsrpSup* indicates the UE supports CSI-RS based cell/beam specific RSRP measurement;  - *csirsrqSup* indicates the UE supports CSI-RS based cell/beam specific RSRQ measurement. |
| ***ten-ms-unit-ResponseTime***  This field, if present, indicates that the target device supports the enumerated value '*ten-milli-seconds*' in the IE *ResponseTime* in IE *CommonIEsRequestLocationInformation*. |
| ***scheduledLocationRequestSupported***  This field, if present, indicates that the target device supports scheduled location requests – i.e., supports the IE *ScheduledLocationTime* in IE *CommonIEsRequestLocationInformation* – and the time base(s) supported for the scheduled location time. |
| ***periodicReportingIntervalMsSupport***  This field, if present, indicates that the target device supports millisecond periodic reporting intervals for location information – i.e., supports the subfield *reportingIntervalMs* of the IE *PeriodicalReportingCriteriaExt* in IE *CommonIEsRequestLocationInformation* – and the minimum millisecond report interval supported for the periodic reporting. |

#### 6.5.9.5 NR E-CID Capability Information Request

#### – *NR-ECID-RequestCapabilities*

The IE *NR-ECID-RequestCapabilities* is used by the location server to request the capability of the target device to support NR E-CID and to request NR E-CID positioning capabilities from a target device.

-- ASN1START

NR-ECID-RequestCapabilities-r16 ::= SEQUENCE {

...

}

-- ASN1STOP

#### 6.5.9.6 NR E-CID Error Elements

#### – *NR-ECID-Error*

The IE *NR-ECID-Error* is used by the location server or target device to provide NR E-CID error reasons to the target device or location server, respectively.

-- ASN1START

NR-ECID-Error-r16 ::= CHOICE {

locationServerErrorCauses-r16 NR-ECID-LocationServerErrorCauses-r16,

targetDeviceErrorCauses-r16 NR-ECID-TargetDeviceErrorCauses-r16,

...

}

-- ASN1STOP

#### – *NR-ECID-LocationServerErrorCauses*

The IE *NR-ECID-LocationServerErrorCauses* is used by the location server to provide NR E-CID error reasons to the target device.

-- ASN1START

NR-ECID-LocationServerErrorCauses-r16 ::= SEQUENCE {

cause-r16 ENUMERATED { undefined,

...

},

...

}

-- ASN1STOP

#### – *NR-ECID-TargetDeviceErrorCauses*

The IE *NR-ECID-TargetDeviceErrorCauses* is used by the target device to provide NR E-CID error reasons to the location server.

-- ASN1START

NR-ECID-TargetDeviceErrorCauses-r16 ::= SEQUENCE {

cause-r16 ENUMERATED { undefined,

requestedMeasurementNotAvailable,

notAllrequestedMeasurementsPossible,

...

},

ss-RSRPMeasurementNotPossible-r16 NULL OPTIONAL,

ss-RSRQMeasurementNotPossible-r16 NULL OPTIONAL,

csi-RSRPMeasurementNotPossible-r16 NULL OPTIONAL,

csi-RSRQMeasurementNotPossible-r16 NULL OPTIONAL,

...,

[[

remoteUE-Indication-r18 ENUMERATED {true} OPTIONAL -- Cond NR

]]

}

-- ASN1STOP

| Conditional presence | Explanation |
| --- | --- |
| *NR* | This field is optionally present, need OR, for NR access. Otherwise it is not present. |

| *NR-ECID-TargetDeviceErrorCauses* field descriptions |
| --- |
| ***cause***  This field provides a NR E-CID specific error cause. If the cause value is 'notAllRequestedMeasurementsPossible', the target device was not able to provide all requested NR E-CID measurements (but may be able to provide some measurements). In this case, the target device should include any of the *ss-RSRPMeasurementNotPossible*, *ss-RSRQMeasurementNotPossible*, *csi-RSRPMeasurementNotPossible*, or *csi-RSRQMeasurementNotPossible* fields, as applicable. |
| ***remoteUE-Indication***  This field indicates whether the target device in NR access is configured as a L2 U2N Remote UE. |

### 6.5.10 NR DL-TDOA Positioning

This clause defines the information elements for NR downlink TDOA positioning (TS 38.305 [40]).

#### 6.5.10.1 NR DL-TDOA Assistance Data

#### – *NR-DL-TDOA-ProvideAssistanceData*

The IE *NR-DL-TDOA-ProvideAssistanceData* is used by the location server to provide assistance data to enable UE‑assisted and UE-based NR DL-TDOA. It may also be used to provide NR DL-TDOA positioning specific error reason.

-- ASN1START

NR-DL-TDOA-ProvideAssistanceData-r16 ::= SEQUENCE {

nr-DL-PRS-AssistanceData-r16 NR-DL-PRS-AssistanceData-r16 OPTIONAL, -- Need ON

nr-SelectedDL-PRS-IndexList-r16 NR-SelectedDL-PRS-IndexList-r16 OPTIONAL, -- Need ON

nr-PositionCalculationAssistance-r16

NR-PositionCalculationAssistance-r16

OPTIONAL, -- Cond UEB

nr-DL-TDOA-Error-r16 NR-DL-TDOA-Error-r16 OPTIONAL, -- Need ON

...,

[[

nr-On-Demand-DL-PRS-Configurations-r17

NR-On-Demand-DL-PRS-Configurations-r17

OPTIONAL, -- Need ON

nr-On-Demand-DL-PRS-Configurations-Selected-IndexList-r17

NR-On-Demand-DL-PRS-Configurations-Selected-IndexList-r17 OPTIONAL, -- Need ON

assistanceDataValidityArea-r17 AreaID-CellList-r17 OPTIONAL -- Need ON

]],

[[

nr-PeriodicAssistData-r18 NR-PeriodicAssistData-r18 OPTIONAL -- Cond CtrTrans

]]

}

-- ASN1STOP

| Conditional presence | Explanation |
| --- | --- |
| *UEB* | The field is optionally present, need ON, for UE based NR DL-TDOA; otherwise it is not present. |
| *CtrTrans* | The field is mandatory present in the control transaction of a periodic assistance data delivery session as described in clauses 5.2.1a and 5.2.2a, for UE based NR DL-TDOA. Otherwise it is not present. |

|  |
| --- |
| *NR-DL-TDOA-ProvideAssistanceData* field descriptions |
| ***nr-DL-PRS-AssistanceData***  This field specifies the assistance data reference and neighbour TRPs and provides the DL-PRS configuration for the TRPs.  Note, if this field is absent but the *nr-SelectedDL-PRS-IndexList* field is present, the *nr-DL-PRS-AssistanceData* may be provided in IE *NR-Multi-RTT-ProvideAssistanceData*, *NR-DL-AoD-ProvideAssistanceData*, or *NR-AI-ML-PositioningProvideAssistanceData*. |
| ***nr-SelectedDL-PRS-IndexList***  This field specifies the DL-PRS Resources which are applicable for this *NR-DL-TDOA-ProvideAssistanceData* message. |
| ***nr-PositionCalculationAssistance***  This field provides position calculation assistance data for UE-based mode. |
| ***nr-DL-TDOA-Error***  This field provides DL-TDOA error reasons. |
| ***nr-On-Demand-DL-PRS-Configurations***  This field provides a set of available DL-PRS configurations which can be requested by the target device on-demand.  NOTE 1: Void  NOTE 2: If this field is absent but the *nr-On-Demand-DL-PRS-Configurations-Selected-IndexList* is present, the *nr-On-Demand-DL-PRS-Configurations* may be provided in IE *NR-Multi-RTT-ProvideAssistanceData,* *NR-DL-AoD-ProvideAssistanceData*, or *NR-AI-ML-PositioningProvideAssistanceData*. |
| ***nr-On-Demand-DL-PRS-Configurations-Selected-IndexList***  This field specifies the selected available on-demand DL-PRS configurations which are applicable for this *NR-DL-TDOA-ProvideAssistanceData message*. |
| ***assistanceDataValidityArea***  This field specifies the network area for which this *NR-DL-TDOA-ProvideAssistanceData* is valid. |
| ***nr-PeriodicAssistData***  This field specifies the control parameters for a periodic assistance data delivery session (e.g., interval and duration) for UE‑based carrier phase positioning. |

Editor's Note: It is FFS whether DL-PRS and on-demand PRS assistance data are applicable to AI/ML positioning.

#### 6.5.10.2 NR DL-TDOA Assistance Data Request

#### – *NR-DL-TDOA-RequestAssistanceData*

The IE *NR-DL-TDOA-RequestAssistanceData* is used by the target device to request assistance data from a location server.

-- ASN1START

NR-DL-TDOA-RequestAssistanceData-r16 ::= SEQUENCE {

nr-PhysCellID-r16 NR-PhysCellID-r16 OPTIONAL,

nr-AdType-r16 BIT STRING { dl-prs (0),

posCalc (1) } (SIZE (1..8)),

...,

[[

nr-PosCalcAssistanceRequest-r17 BIT STRING { trpLoc (0),

beamInfo (1),

rtdInfo (2),

losNlosInfo (3),

trpTEG-Info (4),

nr-IntegrityBounds-r18 (5),

pruInfo-r18 (6)

} (SIZE (1..8)) OPTIONAL,

nr-on-demand-DL-PRS-Request-r17 NR-On-Demand-DL-PRS-Request-r17 OPTIONAL,

nr-DL-PRS-ExpectedAoD-or-AoA-Request-r17

ENUMERATED { eAoD, eAoA } OPTIONAL,

pre-configured-AssistanceDataRequest-r17

ENUMERATED { true } OPTIONAL

]],

[[

nr-PeriodicAssistDataReq-r18 NR-PeriodicAssistDataReq-r18 OPTIONAL, -- Cond PerADReq

nr-IntegrityAssistanceRequest-r18 BIT STRING {

serviceParameters (0),

serviceAlert (1),

riskParameters (2),

integrityParaTRP-Loc (3),

integrityParaBeamInfo (4),

integrityParaRTD-Info (5)

} (SIZE (1..8)) OPTIONAL

]]

}

-- ASN1STOP

| Conditional presence | Explanation |
| --- | --- |
| *PerADReq* | This field is mandatory present if the target device requests periodic NR assistance data delivery. This field may only be included if '*pruInfo*' bit in  *nr-PosCalcAssistanceRequest* is set to '1'. |

|  |
| --- |
| *NR-DL-TDOA-RequestAssistanceData* field descriptions |
| ***nr-PhysCellID***  This field specifies the NR physical cell identity of the current primary cell of the target device. |
| ***nr-AdType***  This field indicates the requested assistance data. *dl-prs* means requested assistance data is *nr-DL-PRS-AssistanceData*, *posCalc* means requested assistance data is *nr-PositionCalculationAssistance* for UE based positioning. |
| ***nr-PosCalcAssistanceRequest***  This field indicates the Position Calculation Assistance Data requested. This is represented by a bit string, with a one‑value at the bit position means the particular assistance data is requested; a zero‑value means not requested.  - bit 0 indicates whether the field *nr-TRP-LocationInfo* in IE *NR-PositionCalculationAssistance* is requested or not;  - bit 1 indicates whether the field *nr-DL-PRS-BeamInfo* in IE *NR-PositionCalculationAssistance* is requested or not;  - bit 2 indicates whether the field *nr-RTD-Info* in IE *NR-PositionCalculationAssistance* is requested or not;  - bit 3 indicates whether the field *nr-DL-PRS-Expected-LOS-NLOS-Assistance* in IE *NR-PositionCalculationAssistance* is requested or not;  - bit 4 indicates whether the field *nr-DL-PRS-TRP-TEG-Info* in IE *NR-PositionCalculationAssistance* is requested or not;  - bit 5 together with bit 0 indicates whether the fields *nr-IntegrityTRP-LocationBounds*, *nr-IntegrityDL-PRS-ResourceSetARP-LocationBounds*, *nr-IntegrityDL-PRS-ResourceARP-LocationBounds* in IE *NR-TRP-LocationInfo* are requested or not; bit 5 together with bit 1 indicates whether the field *nr-IntegrityBeamInfoBounds* in IE *NR-DL-PRS-BeamInfo* is requested or not; bit 5 together with the bit 2 indicates whether the field *nr-IntegrityRTD-InfoBounds* in IE *NR-RTD-Info* is requested or not;  - bit 6 indicates whether the field *nr-PRU-DL-Info* in IE *NR-PositionCalculationAssistance* is requested or not.  This field may only be present if the '*posCalc*' bit in *nr-AdType* is set to value '1'. |
| ***nr-on-demand-DL-PRS-Request***  This field indicates the on-demand DL-PRS requested for DL-TDOA. This field may be included when the *dl-prs* bit in *nr-AdType* is set to value '1'. |
| ***nr-DL-PRS-ExpectedAoD-or-AoA-Request***  This field, if present, indicates that the IE *NR-DL-PRS-ExpectedAoD-or-AoA* in *NR-DL-PRS-AssistanceData* is requested. Enumerated value '*eAoD*' indicates that expected AoD information is requested; value '*eAoA*' indicates that expected AoA information is requested.  This field may only be present if the '*dl-prs*' bit in *nr-AdType* is set to value '1'. |
| ***pre-configured-AssistanceDataRequest***  This field, if present, indicates that the target device requests pre-configured assistance data with area validity. |
| ***nr-PeriodicAssistDataReq***  This field indicates the control parameters for a periodic assistance data delivery session (e.g., interval and duration) for UE‑based carrier phase positioning. |
| ***nr-IntegrityAssistanceRequest***  This field indicates the Integrity Assistance Data requested. This is represented by a bit string, with a one‑value at the bit position means the particular assistance data is requested; a zero‑value means not requested.  - bit 0 indicates whether the field *nr-IntegrityServiceParameters* in IE *NR-PositionCalculationAssistance* is requested or not;  - bit 1 indicates whether the field *nr-IntegrityServiceAlert* in IE *NR-PositionCalculationAssistance* is requested or not;  - bit 2 indicates whether the field *nr-IntegrityRiskParameters* in IE *NR-PositionCalculationAssistance* is requested or not;  - bit 3 indicates whether the field *nr-IntegrityParametersTRP-LocationInfo* in IE *NR-PositionCalculationAssistance* is requested or not;  - bit 4 indicates whether the field *nr-IntegrityParametersDL-PRS-BeamInfo* in IE *NR-PositionCalculationAssistance* is requested or not;  - bit 5 indicates whether the field *nr-IntegrityParametersRTD-Info* in IE *NR-PositionCalculationAssistance* is requested or not. |

#### 6.5.10.3 NR DL-TDOA Location Information

#### – *NR-DL-TDOA-ProvideLocationInformation*

The IE *NR-DL-TDOA-ProvideLocationInformation* is used by the target device to provide NR DL-TDOA location measurements to the location server. It may also be used to provide NR DL-TDOA positioning specific error reason.

-- ASN1START

NR-DL-TDOA-ProvideLocationInformation-r16 ::= SEQUENCE {

nr-DL-TDOA-SignalMeasurementInformation-r16

NR-DL-TDOA-SignalMeasurementInformation-r16

OPTIONAL,

nr-dl-tdoa-LocationInformation-r16 NR-DL-TDOA-LocationInformation-r16

OPTIONAL,

nr-DL-TDOA-Error-r16 NR-DL-TDOA-Error-r16 OPTIONAL,

...,

[[

nr-DL-TDOA-SignalMeasurementInstances-r17

SEQUENCE (SIZE (1..maxMeasInstances-r17)) OF

NR-DL-TDOA-SignalMeasurementInformation-r16

OPTIONAL, -- Cond batchUEA

nr-DL-TDOA-LocationInformationInstances-r17

SEQUENCE (SIZE (1..maxMeasInstances-r17)) OF

NR-DL-TDOA-LocationInformation-r16

OPTIONAL -- Cond batchUEB

]]

}

-- ASN1STOP

| Conditional presence | Explanation |
| --- | --- |
| *batchUEA* | The field is optionally present if the field *nr-DL-TDOA-SignalMeasurementInformation* is absent; otherwise it is not present. |
| *batchUEB* | The field is optionally present if the field *nr-dl-tdoa-LocationInformation* is absent; otherwise it is not present. |

#### 6.5.10.4 NR DL-TDOA Location Information Elements

#### – *NR-DL-TDOA-SignalMeasurementInformation*

The IE *NR-DL-TDOA-SignalMeasurementInformation* is used by the target device to provide NR DL-TDOA measurements to the location server.

NOTE 1: The *dl-PRS-ReferenceInfo* defines the "RSTD reference" TRP. The *nr-RSTD's* and *nr-RSTD-ResultDiff*'s in *nr-DL-TDOA-MeasList* are provided relative to the "RSTD reference" TRP.

NOTE 2: The "RSTD reference" TRP may or may not be the same as the "assistance data reference" TRP provided by *nr-DL-PRS-ReferenceInfo* in IE *NR-DL-PRS-AssistanceData.*

NOTE 3: The target device includes a value of zero for the *nr-RSTD* and *nr-RSTD-ResultDiff* of the "RSTD reference" TRP in *nr-DL-TDOA-MeasList*.

-- ASN1START

NR-DL-TDOA-SignalMeasurementInformation-r16 ::= SEQUENCE {

dl-PRS-ReferenceInfo-r16 DL-PRS-ID-Info-r16,

nr-DL-TDOA-MeasList-r16 NR-DL-TDOA-MeasList-r16,

...,

[[

nr-UE-RxTEG-TimingErrorMargin-r17 TEG-TimingErrorMargin-r17 OPTIONAL -- Cond UERxTEG

]]

}

NR-DL-TDOA-MeasList-r16 ::= SEQUENCE (SIZE(1..nrMaxTRPs-r16)) OF NR-DL-TDOA-MeasElement-r16

NR-DL-TDOA-MeasElement-r16 ::= SEQUENCE {

dl-PRS-ID-r16 INTEGER (0..255),

nr-PhysCellID-r16 NR-PhysCellID-r16 OPTIONAL,

nr-CellGlobalID-r16 NCGI-r15 OPTIONAL,

nr-ARFCN-r16 ARFCN-ValueNR-r15 OPTIONAL,

nr-DL-PRS-ResourceID-r16 NR-DL-PRS-ResourceID-r16 OPTIONAL,

nr-DL-PRS-ResourceSetID-r16 NR-DL-PRS-ResourceSetID-r16 OPTIONAL,

nr-TimeStamp-r16 NR-TimeStamp-r16,

nr-RSTD-r16 CHOICE {

k0-r16 INTEGER (0..1970049),

k1-r16 INTEGER (0..985025),

k2-r16 INTEGER (0..492513),

k3-r16 INTEGER (0..246257),

k4-r16 INTEGER (0..123129),

k5-r16 INTEGER (0..61565),

...,

kMinus6-r18 INTEGER (0..126083073),

kMinus5-r18 INTEGER (0..63041537),

kMinus4-r18 INTEGER (0..31520769),

kMinus3-r18 INTEGER (0..15760385),

kMinus2-r18 INTEGER (0..7880193),

kMinus1-r18 INTEGER (0..3940097)

},

nr-AdditionalPathList-r16 NR-AdditionalPathList-r16 OPTIONAL,

nr-TimingQuality-r16 NR-TimingQuality-r16,

nr-DL-PRS-RSRP-Result-r16 INTEGER (0..126) OPTIONAL,

nr-DL-TDOA-AdditionalMeasurements-r16

NR-DL-TDOA-AdditionalMeasurements-r16 OPTIONAL,

...,

[[

nr-UE-Rx-TEG-ID-r17 INTEGER (0..maxNumOfRxTEGs-1-r17) OPTIONAL,

nr-DL-PRS-FirstPathRSRP-Result-r17 INTEGER (0..126) OPTIONAL,

nr-los-nlos-Indicator-r17 CHOICE {

perTRP-r17 LOS-NLOS-Indicator-r17,

perResource-r17 LOS-NLOS-Indicator-r17

} OPTIONAL,

nr-AdditionalPathListExt-r17 NR-AdditionalPathListExt-r17 OPTIONAL,

nr-DL-TDOA-AdditionalMeasurementsExt-r17

NR-DL-TDOA-AdditionalMeasurementsExt-r17 OPTIONAL

]],

[[

nr-MeasBasedOnAggregatedResources-r18 ENUMERATED {true} OPTIONAL,

nr-AggregatedDL-PRS-ResourceInfo-List-r18 SEQUENCE (SIZE (2.. 3)) OF

NR-AggregatedDL-PRS-ResourceInfo-Element-r18 OPTIONAL,

nr-RSCPD-r18 INTEGER (0..3599) OPTIONAL,

nr-PhaseQuality-r18 NR-PhaseQuality-r18 OPTIONAL,

nr-RSCPD-AddMeasurementSamples-r18 SEQUENCE (SIZE (1..nrNumOfSamples-1-r18 )) OF

NR-RSCPD-AdditionalMeasurementSamplesElement-r18 OPTIONAL,

nr-ReportDL-PRS-MeasBasedOnSingleOrMultiHopRx-r18

ENUMERATED { singleHop, multipleHop } OPTIONAL

]]

}

NR-DL-TDOA-AdditionalMeasurements-r16 ::= SEQUENCE (SIZE (1..3)) OF

NR-DL-TDOA-AdditionalMeasurementElement-r16

NR-DL-TDOA-AdditionalMeasurementsExt-r17 ::= SEQUENCE (SIZE (1..maxAddMeasTDOA-r17)) OF

NR-DL-TDOA-AdditionalMeasurementElement-r16

NR-DL-TDOA-AdditionalMeasurementElement-r16 ::= SEQUENCE {

nr-DL-PRS-ResourceID-r16 NR-DL-PRS-ResourceID-r16 OPTIONAL,

nr-DL-PRS-ResourceSetID-r16 NR-DL-PRS-ResourceSetID-r16 OPTIONAL,

nr-TimeStamp-r16 NR-TimeStamp-r16,

nr-RSTD-ResultDiff-r16 CHOICE {

k0-r16 INTEGER (0..8191),

k1-r16 INTEGER (0..4095),

k2-r16 INTEGER (0..2047),

k3-r16 INTEGER (0..1023),

k4-r16 INTEGER (0..511),

k5-r16 INTEGER (0..255),

...,

kMinus6-r18 INTEGER (0..524224),

kMinus5-r18 INTEGER (0..262112),

kMinus4-r18 INTEGER (0..131056),

kMinus3-r18 INTEGER (0..65528),

kMinus2-r18 INTEGER (0..32764),

kMinus1-r18 INTEGER (0..16382)

},

nr-TimingQuality-r16 NR-TimingQuality-r16,

nr-DL-PRS-RSRP-ResultDiff-r16 INTEGER (0..61) OPTIONAL,

nr-AdditionalPathList-r16 NR-AdditionalPathList-r16 OPTIONAL,

...,

[[

nr-UE-Rx-TEG-ID-r17 INTEGER (0..maxNumOfRxTEGs-1-r17) OPTIONAL,

nr-DL-PRS-FirstPathRSRP-ResultDiff-r17

INTEGER (0..61) OPTIONAL,

nr-los-nlos-IndicatorPerResource-r17

LOS-NLOS-Indicator-r17 OPTIONAL,

nr-AdditionalPathListExt-r17 NR-AdditionalPathListExt-r17 OPTIONAL

]],

[[

nr-MeasBasedOnAggregatedResources-r18 ENUMERATED {true} OPTIONAL,

nr-AggregatedDL-PRS-ResourceInfo-List-r18 SEQUENCE (SIZE (2.. 3)) OF

NR-AggregatedDL-PRS-ResourceInfo-Element-r18 OPTIONAL,

nr-RSCPD-r18 INTEGER (0..3599) OPTIONAL,

nr-PhaseQuality-r18 NR-PhaseQuality-r18 OPTIONAL,

nr-RSCPD-AdditionalMeasurementsAddSamples-r18

SEQUENCE (SIZE (1..nrNumOfSamples-1-r18 )) OF

NR-RSCPD-AdditionalMeasurementSamplesElement-r18 OPTIONAL,

nr-ReportDL-PRS-MeasBasedOnSingleOrMultiHopRx-r18

ENUMERATED { singleHop, multipleHop } OPTIONAL

]]

}

NR-RSCPD-AdditionalMeasurementSamplesElement-r18 ::= SEQUENCE {

nr-RSCPD-r18 INTEGER (0..3599) OPTIONAL,

nr-PhaseQuality-r18 NR-PhaseQuality-r18 OPTIONAL,

nr-TimeStamp-r18 NR-TimeStamp-r16 OPTIONAL,

...

}

-- ASN1STOP

| Conditional presence | Explanation |
| --- | --- |
| *UERxTEG* | The field is optionally present, need OP, if the field *nr-UE-Rx-TEG-ID* is present; otherwise it is not present. |

|  |
| --- |
| *NR-DL-TDOA-SignalMeasurementInformation* field descriptions |
| ***nr-UE-RxTEG-TimingErrorMargin***  This field specifies the UE Rx TEG timing error margin value for all the UE Rx TEGs within one *NR-DL-TDOA-SignalMeasurementInformation*. If the *nr-UE-Rx-TEG-ID* is present and this field is absent, the receiver should consider the UE Rx TEG timing error margin value to be the maximum applicable value as defined in TS 38.133 [46]. |
| ***dl-PRS-ID***  This field is used along with a DL-PRS Resource Set ID and a DL-PRS Resources ID to uniquely identify a DL-PRS Resource. This ID can be associated with multiple DL-PRS Resource Sets associated with a single TRP.  Each TRP should only be associated with one such ID. |
| ***nr-PhysCellID***  This field specifies the physical cell identity of the associated TRP, as defined in TS 38.331 [35]. |
| ***nr-CellGlobalID***  This field specifies the NCGI, the globally unique identity of a cell in NR, of the associated TRP, as defined in TS 38.331 [35]. |
| ***nr-ARFCN***  This field specifies the NR-ARFCN of the TRP's CD-SSB (as defined in TS 38.300 [47]) corresponding to *nr-PhysCellID*. |
| ***nr-TimeStamp***  This field specifies the time instance at which the TOA, RSCP (if included) and DL PRS-RSRP/RSRPP (if included) measurement is performed. The *nr-SFN,* *nr-Slot* and *nr-Symbol* (if included) in IE *NR-TimeStamp* correspond to the TRP provided in *dl-PRS-ReferenceInfo* as specified in TS 38.214 [45]. Note, the TOA measurement refers to the TOA of this neighbour TRP or the reference TRP, as applicable, used to determine the *nr-RSTD* or *nr-RSTD-ResultDiff*. |
| ***nr-RSTD***  This field specifies the relative timing difference between this neighbour TRP and the DL-PRS reference TRP, as defined in TS 38.215 [36]. Mapping of the measured quantity is defined as in TS 38.133 [46]. |
| ***nr-AdditionalPathList***  This field specifies one or more additional detected path timing values for the TRP or resource, relative to the path timing used for determining the *nr-RSTD* value. If this field was requested but is not included, it means the UE did not detect any additional path timing values. If this field is present, the field *nr-AdditionalPathListExt* shall be absent. |
| ***nr-TimingQuality***  This field specifies the target device′s best estimate of the quality of the TOA measurement. Note, the TOA measurement refers to the TOA of this neighbour TRP or the reference TRP, as applicable, used to determine the *nr-RSTD* or *nr-RSTD-ResultDiff*. |
| ***nr-DL-PRS-RSRP-Result***  This field specifies the NR DL-PRS reference signal received power (DL PRS-RSRP) measurement, as defined in TS 38.215 [36]. The mapping of the quantity is defined as in TS 38.133 [46]. |
| ***nr-DL-TDOA-AdditionalMeasurements***  This field provides up to 3 additional RSTD measurements per pair of TRPs, with each measurement between a different pair of DL-PRS Resources or DL-PRS Resource Sets of the DL-PRS for those TRPs [45].  If this field is present, the field *nr-DL-TDOA-AdditionalMeasurementsExt* shall be absent. |
| ***nr-UE-Rx-TEG-ID***  This field provides the ID of the UE Rx TEG associated with the TOA measurement. Note, the TOA measurement refers to the TOA of this neighbour TRP or the reference TRP, as applicable, used to determine the *nr-RSTD* or *nr-RSTD-ResultDiff*. When different UE Rx TEGs for RSTD measurements are requested, the maximum number of reported RSTD measurements associated with different DL-PRS Resources per UE Rx TEG per target TRP is 4. |
| ***nr-DL-PRS-FirstPathRSRP-Result***  This field specifies the NR DL-PRS reference signal received path power (DL PRS-RSRPP) of the first detected path in time, as defined in TS 38.215 [36]. The mapping of the measured quantity is defined as in TS 38.133 [46]. |
| ***nr-los-nlos-Indicator***  This field specifies the target device's best estimate of the LOS or NLOS of the TOA measurement for the TRP or resource. Note, the TOA measurement refers to the TOA of this neighbour TRP or the reference TRP, as applicable, used to determine the *nr-RSTD* or *nr-RSTD-ResultDiff*.  This field also applies to specify the target device's best estimate of the LOS or NLOS of the RSCP measurement for the TRP or resource. Note, the RSCP measurement refers to the RSCP of this neighbour TRP or the reference TRP, as applicable, used to determine the *nr-RSCPD*.  NOTE: If the requested type or granularity in *nr-los-nlos-IndicatorRequest* is not possible, the target device may provide a different type and granularity for the estimated *LOS-NLOS-Indicator.* |
| ***nr-AdditionalPathListExt***  This field provides up to 8 additional detected path timing values for the TRP or resource, relative to the path timing used for determining the *nr-RSTD* value. If this field was requested but is not included, it means the UE did not detect any additional path timing values. If this field is present, the field *nr-AdditionalPathList* shall be absent. |
| ***nr-DL-TDOA-AdditionalMeasurementsExt***  This field, in addition to the measurements provided in *NR-DL-TDOA-MeasElement*, provides TOA measurements of up to 4 DL-PRS Resources of a TRP with different UE Rx TEGs. For a certain DL-PRS Resource, there can be up to 8 TOA measurement results with respect to different Rx TEGs.  If this field is present, the field *nr-DL-TDOA-AdditionalMeasurements* shall be absent. |
| ***nr-MeasBasedOnAggregatedResources***  This field indicates whether the RSTD measurement, RSRP measurement (if included), and RSRPP measurement (if included) is based on aggregated DL-PRS Resources. |
| ***nr-AggregatedDL-PRS-ResourceInfo-List***  This field provides the DL-PRS Resource Set IDs which are used for the aggregated RSTD, RSRP, or RSRPP measurement results. This field is optionally present if the field *nr-MeasBasedOnAggregatedResources* is present; otherwise, it is not present. If the field is present, the field *nr-DL-PRS-ResourceID* and *nr-DL-PRS-ResourceSetID* should not be included, and the *dl-PRS-ID* in IE *NR-DL-TDOA-MeasElement* shall be ignored by a receiver. The a*ggregatedDL-PRS-ID* in the *nr-AggregatedDL-PRS-ResourceInfo-List* is always provided for the first measurement when *nr-AggregatedDL-PRS-ResourceInfo-List* is included in *NR-DL-TDOA-MeasElement*. The a*ggregatedDL-PRS-ID* is not present in the *nr-AggregatedDL-PRS-ResourceInfo-List* when *nr-AggregatedDL-PRS-ResourceInfo-List* is included in *NR-DL-TDOA-AdditionalMeasurementElement*. |
| ***nr-RSCPD***  This field specifies the NR DL reference signal carrier phase difference measurement, as defined in TS 38.215 [36]. Mapping of the measured quantity is defined as in TS 38.133 [46]. This neighbour TRP measurement is made using DL-PRS Resources from the same PFL as the reference TRP measurement. |
| ***nr-PhaseQuality***  This field specifies the target device′s best estimate of the quality of the RSCPD measurement. |
| ***nr-RSCPD-AddMeasurementSamples***  This field, in addition to the *nr-RSCPD* measurements provided in *NR-DL-TDOA-MeasElement*, provides up to 3 RSCPD measurements samples associated with the *nr-RSTD* in *NR-DL-TDOA-MeasElement*. |
| ***nr-ReportDL-PRS-MeasBasedOnSingleOrMultiHopRx***  This field indicates that the reported measurement is based on DL-PRS receive hopping with either single hop or multiple hops. |
| ***nr-RSTD-ResultDiff***  This field provides the additional DL RSTD measurement result relative to *nr-RSTD.* The RSTD value of this measurement is obtained by adding the value of this field to the value of the *nr-RSTD* field. The mapping of the field is defined in TS 38.133 [46]. |
| ***nr-DL-PRS-RSRP-ResultDiff***  This field provides the additional DL-PRS RSRP measurement result relative to *nr-DL-PRS-RSRP-Result.* The DL-PRS RSRP value of this measurement is obtained by adding the value of this field to the value of the *nr-DL-PRS-RSRP-Result* field. The mapping of the field is defined in TS 38.133 [46]. |
| ***nr-DL-PRS-FirstPathRSRP-ResultDiff***  This field specifies the additional NR DL-PRS reference signal received path power (DL PRS-RSRPP) of the first detected path in time relative to *nr-DL-PRS-FirstPathRSRP-Result*. The DL-PRS RSRPP of first path value of this measurement is obtained by adding the value of this field to the value of the *nr-DL-PRS-FirstPathRSRP-Result* field. The mapping of the field is defined in TS 38.133 [46]. |
| ***nr-los-nlos-IndicatorPerResource***  This field specifies the target device's best estimate of the LOS or NLOS of the TOA measurement for the resource. Note, the TOA measurement refers to the TOA of this neighbour TRP or the reference TRP, as applicable, used to determine the *nr-RSTD* or *nr-RSTD-ResultDiff*.  This field may only be present if the field *nr-LOS-NLOS-Indicator* choice indicates *perResource*. |
| ***nr-RSCPD-AdditionalMeasurementsAddSamples***  This field, in addition to the *nr-RSCPD* measurement provided in *NR-DL-TDOA-AdditionalMeasurementElement*, provides up to 3 RSCPD measurement samples associated with the RSTD measurement in *NR-DL-TDOA-AdditionalMeasurementElement.* |

#### *– NR-DL-TDOA-LocationInformation*

The IE *NR-DL-TDOA-LocationInformation* is included by the target device when location information derived using NR DL-TDOA is provided to the location server.

-- ASN1START

NR-DL-TDOA-LocationInformation-r16 ::= SEQUENCE {

measurementReferenceTime-r16 CHOICE {

systemFrameNumber-r16 NR-TimeStamp-r16,

utc-time-r16 UTCTime,

...

} OPTIONAL,

...,

[[

locationCoordinates-r17 LocationCoordinates OPTIONAL, -- Cond batch1

locationSource-r17 LocationSource-r13 OPTIONAL -- Cond batch2

]]

}

-- ASN1STOP

| Conditional presence | Explanation |
| --- | --- |
| *batch1* | The field is mandatory present if the field *nr-DL-TDOA-LocationInformationInstances* is present in IE *NR-DL-TDOA-ProvideLocationInformation*; otherwise it is not present. |
| *batch2* | The field is optionally present, need ON, if the field *nr-DL-TDOA-LocationInformationInstances* is present in IE *NR-DL-TDOA-ProvideLocationInformation*; otherwise it is not present. |

|  |
| --- |
| *NR-DL-TDOA-LocationInformation* field descriptions |
| ***measurementReferenceTime***  This field specifies the time for which the location estimate is valid. |
| ***locationCoordinates***  This field provides a location estimate using one of the geographic shapes defined in TS 23.032 [15]. NOTE 1. |
| ***locationSource***  This field provides the source positioning technology for the location estimate. NOTE 1. |

NOTE 1: In the case of locationCoordinates for multiple NR positioning methods are provided, the locationCoordinates and locationSource shall be present in only one of NR-DL-TDOA-ProvideLocationInformation or NR-DL-AoD-ProvideLocationInformation.

#### 6.5.10.5 NR DL-TDOA Location Information Request

#### – *NR-DL-TDOA-RequestLocationInformation*

The IE *NR-DL-TDOA-RequestLocationInformation* is used by the location server to request NR DL-TDOA location measurements from a target device.

-- ASN1START

NR-DL-TDOA-RequestLocationInformation-r16 ::= SEQUENCE {

nr-DL-PRS-RstdMeasurementInfoRequest-r16 ENUMERATED { true } OPTIONAL,-- Need ON

nr-RequestedMeasurements-r16 BIT STRING { prsrsrpReq (0),

firstPathRsrpReq-r17 (1),

dl-PRS-RSCPD-Request-r18 (2)

} (SIZE(1..8)),

nr-AssistanceAvailability-r16 BOOLEAN,

nr-DL-TDOA-ReportConfig-r16 NR-DL-TDOA-ReportConfig-r16 OPTIONAL, -- Need ON

additionalPaths-r16 ENUMERATED { requested } OPTIONAL, -- Need ON

...,

[[

nr-UE-RxTEG-Request-r17 ENUMERATED { requested } OPTIONAL, -- Need ON

nr-los-nlos-IndicatorRequest-r17 SEQUENCE {

type-r17 LOS-NLOS-IndicatorType1-r17,

granularity-r17 LOS-NLOS-IndicatorGranularity1-r17,

...

} OPTIONAL, -- Need ON

additionalPathsExt-r17 ENUMERATED { requested } OPTIONAL, -- Need ON

additionalPathsDL-PRS-RSRP-Request-r17 ENUMERATED { requested } OPTIONAL, -- Need ON

multiMeasInSameReport-r17 ENUMERATED { requested } OPTIONAL -- Need ON

]],

[[

nr-DL-PRS-JointMeasurementRequest-r18 SEQUENCE {

nr-DL-PRS-JointMeasurementRequestedPFL-List-r18 SEQUENCE (SIZE (2..3)) OF

INTEGER (0..nrMaxFreqLayers-1-r16) OPTIONAL -- Need ON

} OPTIONAL, -- Need ON

nr-DL-PRS-RxHoppingRequest-r18 SEQUENCE {

nr-DL-PRS-RxHoppingTotalBandwidth-r18 CHOICE {

fr1 ENUMERATED {mhz40, mhz50, mhz80, mhz100},

fr2 ENUMERATED {mhz100, mhz200, mhz400}

} OPTIONAL -- Need ON

} OPTIONAL -- Need ON

]]

}

NR-DL-TDOA-ReportConfig-r16 ::= SEQUENCE {

maxDL-PRS-RSTD-MeasurementsPerTRP-Pair-r16 INTEGER (1..4) OPTIONAL, -- Need ON

timingReportingGranularityFactor-r16 INTEGER (0..5) OPTIONAL, -- Need ON

...,

[[

measureSameDL-PRS-ResourceWithDifferentRxTEGs-r17

ENUMERATED { n0, n2, n3, n4, n6, n8, ... }

OPTIONAL, -- Need ON

reducedDL-PRS-ProcessingSamples-r17 ENUMERATED { requested, ... } OPTIONAL, -- Need ON

lowerRxBeamSweepingFactor-FR2-r17 ENUMERATED { requested } OPTIONAL -- Need ON

]],

[[

timingReportingGranularityFactorExt-r18 INTEGER (-6..-1) OPTIONAL, -- Need ON

nr-DL-PRS-MeasurementTimeWindowsConfig-r18

NR-DL-PRS-MeasurementTimeWindowsConfig-r18 OPTIONAL -- Need ON

]]

}

-- ASN1STOP

|  |
| --- |
| *NR-DL-TDOA-RequestLocationInformation* field descriptions |
| ***nr-DL-PRS-RstdMeasurementInfoRequest***  This field indicates whether the target device is requested to report DL-PRS Resource ID(s) or DL-PRS Resource Set ID(s) used for determining the timing of each TRP in RSTD measurements. |
| ***nr-RequestedMeasurements***  This field specifies the NR DL-TDOA measurements requested. This is represented by a bit string, with a one‑value at the bit position means the particular measurement is requested; a zero‑value means not requested. The *dl-PRS-RSCPD-Request* means that the target device is requested to provide DL RSCPD measurement. |
| ***nr-AssistanceAvailability***  This field indicates whether the target device may request additional DL-PRS assistance data from the server. TRUE means allowed and FALSE means not allowed. |
| ***additionalPaths***  This field, if present, indicates that the target device is requested to provide the *nr-AdditionalPathList* in IE *NR-DL-TDOA-SignalMeasurementInformation*. If this field is present, the field *additionalPathsExt* shall be absent. |
| ***nr-UE-RxTEG-Request***  This field, if present, indicates that the target device is requested to provide the *nr-UE-Rx-TEG-ID* in IE *NR-DL-TDOA-SignalMeasurementInformation.* |
| ***nr-los-nlos-IndicatorRequest***  This field, if present, indicates that the target device is requested to provide the indicated type and granularity of the estimated *LOS-NLOS-Indicator* in the *NR-DL-TDOA-SignalMeasurementInformation*. |
| ***additionalPathsExt***  This field, if present, indicates that the target device is requested to provide the *nr-AdditionalPathListExt* in IE *NR-DL-TDOA-SignalMeasurementInformation*. If this field is present, the field *additionalPaths* shall be absent. |
| ***additionalPathsDL-PRS-RSRP-Request***  This field, if present, indicates that the target device is requested to provide the *nr-DL-PRS-RSRPP* for the additional paths in fields *nr-AdditionalPathList* or *nr-AdditionalPathListExt*. |
| ***multiMeasInSameReport***  This field, if present, indicates that the target device is requested to provide multiple measurement instances in a single measurement report; i.e., include the *nr-DL-TDOA-SignalMeasurementInstances* (in the case of UE-assisted mode is requested) or *nr-DL-TDOA-LocationInformationInstances* (in the case of UE-based mode is requested) in IE *NR-DL-TDOA-ProvideLocationInformation.* |
| ***nr-DL-PRS-JointMeasurementRequest***  This field, if present, indicates that the target device is requested to perform joint measurement across aggregated PFLs. |
| ***nr-DL-PRS-JointMeasurementRequestedPFL-List***  This field, if present, indicates the target device is requested to perform joint measurements on the indicated two or three PFLs. Value 0 corresponds to the first frequency layer provided in *nr-DL-PRS-AssistanceDataList*, value 1 to the second frequency layer in *nr-DL-PRS-AssistanceDataList*, and so on. |
| ***nr-DL-PRS-RxHoppingRequest***  This field, if present, indicates that the target device is requested to use DL-PRS Rx hopping for performing RSTD, RSRP (if requested in *nr-RequestedMeasurements*), or RSRPP measurements (if requested in *nr-RequestedMeasurements*) and report the hopping information used for performing the measurements. This field is not included when *dl-PRS-RSCPD-Request* or *nr-DL-PRS-JointMeasurementRequest* is included. |
| ***nr-DL-PRS-RxHoppingTotalBandwidth***  This field, if present, indicates the total bandwidth in MHz across all hops for the DL-PRS measurement. If the configured value *nr-DL-PRS-RxHoppingTotalBandwidth* is larger than the configured DL-PRS bandwidth in the provided assistance data, the UE shall assume that the actual nr-*DL-PRS-RxHoppingTotalBandwidth* is equal to the width of the configured DL-PRS in the provided assistance data. |
| ***maxDL-PRS-RSTD-MeasurementsPerTRP-Pair***  This field specifies the maximum number of DL-PRS RSTD measurements per pair of TRPs. The maximum number is defined across all Positioning Frequency Layers. When requested for aggregated measurements by the location server, this field specifies the maximum number of aggregated DL-PRS RSTD measurements per pair of TRPs. The maximum number is defined across all Positioning Frequency Layers. |
| ***timingReportingGranularityFactor, timingReportingGranularityFactorExt***  This field specifies the recommended reporting granularity for the DL RSTD measurements. Value (0..5) corresponds to (*k0*..*k5*) and value (-6..-1) corresponds to (*kMinus6*..*kMinus1*) used for *nr-RSTD* and *nr-RSTD-ResultDiff* in *NR-DL-TDOA-MeasElement*. The UE may select a different granularity value for *nr-RSTD* and *nr-RSTD-ResultDiff*. The *timingReportingGranularityFactorExt* should not be included by the location server and shall be ignored by the target device if *timingReportingGranularityFactor* is included.The *timingReportingGranularityFactor* should not be included by the location server and shall be ignored by the target device if *timingReportingGranularityFactorExt* is included. |
| ***measureSameDL-PRS-ResourceWithDifferentRxTEGs***  This field, if present, indicates that the target device is requested to measure the same DL-PRS Resource of a TRP with *N* different UE Rx TEGs. Enumerated value '*n0*' indicates that the number *N* of different UE Rx TEGs to measure the same DL-PRS Resource can be determined by the target device, value '*n2*' indicates that the target device is requested to measure the same DL-PRS Resource of a TRP with 2 different UE Rx TEGs, value '*n3*' indicates that the target device is requested to measure the same DL-PRS Resource of a TRP with 3 different UE Rx TEGs, and so on.  If this field is present, the field *nr-UE-RxTEG-Request* should also be present. When the location server requests aggregated measurements, the target device is requested to measure the same aggregated DL-PRS Resources of a TRP with N different UE Rx TEGs. |
| ***reducedDL-PRS-ProcessingSamples***  This field, if present and set to '*requested*', indicates that the target device is requested to perform the requested measurements with reduced number of samples (M=1 or M=2) as specified in TS 38.133 [46]. When requested for aggregated measurements by the location server, this field indicates processing of reduced number of samples for the aggregated measurements. |
| ***lowerRxBeamSweepingFactor-FR2***  This field, if present, indicates that the target device is requested to use a lower Rx beam sweeping factor than 8 for FR2 according to UE's capability. When requested for aggregated measurements by the location server, this field indicates that the target device is requested to use a lower Rx beam sweeping factor than 8 for FR2 according to UE's capability for the aggregated measurements. |
| ***nr-DL-PRS-MeasurementTimeWindowsConfig***  This field indicates DL-PRS Resource Set(s) occurring within time window(s) for performing measurements where the time window is indicated by a start time, periodicity, offset and duration. |

#### 6.5.10.6 NR DL-TDOA Capability Information

#### – *NR-DL-TDOA-ProvideCapabilities*

The IE *NR-DL-TDOA-ProvideCapabilities* is used by the target device to indicate its capability to support NR DL-TDOA and to provide its NR DL-TDOA positioning capabilities to the location server.

-- ASN1START

NR-DL-TDOA-ProvideCapabilities-r16 ::= SEQUENCE {

nr-DL-TDOA-Mode-r16 PositioningModes,

nr-DL-TDOA-PRS-Capability-r16 NR-DL-PRS-ResourcesCapability-r16,

nr-DL-TDOA-MeasurementCapability-r16 NR-DL-TDOA-MeasurementCapability-r16,

nr-DL-PRS-QCL-ProcessingCapability-r16 NR-DL-PRS-QCL-ProcessingCapability-r16,

nr-DL-PRS-ProcessingCapability-r16 NR-DL-PRS-ProcessingCapability-r16,

additionalPathsReport-r16 ENUMERATED { supported } OPTIONAL,

periodicalReporting-r16 PositioningModes OPTIONAL,

...,

[[

ten-ms-unit-ResponseTime-r17 PositioningModes OPTIONAL,

nr-PosCalcAssistanceSupport-r17 BIT STRING { trpLocSup (0),

beamInfoSup (1),

rtdInfoSup (2),

trpTEG-InfoSup (3),

nr-IntegritySup-r18 (4),

pruInfoSup-r18 (5)

} (SIZE (1..8)) OPTIONAL,

nr-los-nlos-AssistanceDataSupport-r17 SEQUENCE {

type-r17 LOS-NLOS-IndicatorType2-r17,

granularity-r17 LOS-NLOS-IndicatorGranularity2-r17,

...

} OPTIONAL,

nr-DL-PRS-ExpectedAoD-or-AoA-Sup-r17 BIT STRING { eAoD (0),

eAoA (1)

} (SIZE (1..8)) OPTIONAL,

nr-DL-TDOA-On-Demand-DL-PRS-Support-r17 NR-On-Demand-DL-PRS-Support-r17 OPTIONAL,

nr-los-nlos-IndicatorSupport-r17 SEQUENCE {

type-r17 LOS-NLOS-IndicatorType2-r17,

granularity-r17 LOS-NLOS-IndicatorGranularity2-r17,

...

} OPTIONAL,

additionalPathsExtSupport-r17 ENUMERATED { n4, n6, n8 } OPTIONAL,

scheduledLocationRequestSupported-r17 ScheduledLocationTimeSupportPerMode-r17 OPTIONAL,

nr-dl-prs-AssistanceDataValidity-r17 SEQUENCE {

area-validity-r17 INTEGER (1..maxNrOfAreas-r17) OPTIONAL, ...

} OPTIONAL,

multiMeasInSameMeasReport-r17 ENUMERATED { supported } OPTIONAL,

mg-ActivationRequest-r17 ENUMERATED { supported } OPTIONAL

]],

[[

posMeasGapSupport-r17 ENUMERATED { supported } OPTIONAL

]],

[[

multiLocationEstimateInSameMeasReport-r17 ENUMERATED { supported } OPTIONAL

]],

[[

locationCoordinateTypes-r18 LocationCoordinateTypes OPTIONAL,

periodicAssistanceData-r18 BIT STRING { solicited (0),

unsolicited (1)} (SIZE (1..8)) OPTIONAL,

nr-IntegrityAssistanceSupport-r18 BIT STRING {

serviceParametersSup (0),

serviceAlertSup (1),

riskParametersSup (2),

integrityParaTRP-LocSup (3),

integrityParaBeamInfoSup (4),

integrityParaRTD-InfoSup (5)

} (SIZE (1..8)) OPTIONAL,

nr-DL-TDOA-OnDemandPRS-ForBWA-Support-r18

ENUMERATED { supported } OPTIONAL,

periodicReportingIntervalMsSupport-r18 PeriodicReportingIntervalMsSupportPerMode-r18

OPTIONAL

]]

}

-- ASN1STOP

|  |
| --- |
| *NR-DL-TDOA-ProvideCapabilities* field descriptions |
| ***nr-DL-TDOA-Mode***  This field specifies the NR DL-TDOA mode(s) supported by the target device. |
| ***periodicalReporting***  This field, if present, specifies the positioning modes for which the target device supports *periodicalReporting.* This is represented by a bit string, with a one‑value at the bit position means *periodicalReporting* for the positioning mode is supported; a zero‑value means not supported. If this field is absent, the target device does not support *periodicalReporting* in *CommonIEsRequestLocationInformation*. |
| ***ten-ms-unit-ResponseTime***  This field, if present, specifies the positioning modes for which the target device supports the enumerated value '*ten-milli-seconds*' in the IE *ResponseTime* in IE *CommonIEsRequestLocationInformation*. This is represented by a bit string, with a one‑value at the bit position means '*ten-milli-seconds'* response time unit for the positioning mode is supported; a zero‑value means not supported. If this field is absent, the target device does not support '*ten-milli-seconds'* response time unitin *CommonIEsRequestLocationInformation*. |
| ***nr-PosCalcAssistanceSupport***  This field indicates the Position Calculation Assistance Data supported by the target device for UE-based DL-TDOA. This is represented by a bit string, with a one‑value at the bit position means the particular assistance data is supported; a zero‑value means not supported.  - bit 0 indicates whether the field *nr-TRP-LocationInfo* in IE *NR-PositionCalculationAssistance* is supported or not;  - bit 1 indicates whether the field *nr-DL-PRS-BeamInfo* in IE *NR-PositionCalculationAssistance* is supported or not;  - bit 2 indicates whether the field *nr-RTD-Info* in IE *NR-PositionCalculationAssistance* is supported or not;  - bit 3 indicates whether the field *nr-DL-PRS-TRP-TEG-Info* in IE *NR-PositionCalculationAssistance* is supported or not. The UE can indicate this bit only if the UE supports *prs-ProcessingCapabilityBandList* and any of *maxNrOfDL-PRS-ResourceSetPerTrpPerFrequencyLayer*, *maxNrOfTRP-AcrossFreqs*, *maxNrOfPosLayer*, *maxNrOfDL-PRS-ResourcesPerResourceSet* and *maxNrOfDL-PRS-ResourcesPerPositioningFrequencylayer*. Otherwise, the UE does not include this field;  - bit 4 together with bit 0 indicates whether the fields *nr-IntegrityTRP-LocationBounds*, *nr-IntegrityDL-PRS-ResourceSetARP-LocationBounds*, *nr-IntegrityDL-PRS-ResourceARP-LocationBounds* in IE *NR-TRP-LocationInfo* are supported or not; bit 4 together with bit 1 indicates whether the field *nr-IntegrityBeamInfoBounds* in IE *NR-DL-PRS-BeamInfo* is supported or not; bit 4 together with the bit 2 indicates whether the field *nr-IntegrityRTD-InfoBounds* in IE *NR-RTD-Info* is supported or not;  - bit 5 indicates whether the field *nr-PRU-DL-Info* in IE *NR-PositionCalculationAssistance* is supported or not. |
| ***nr-los-nlos-AssistanceDataSupport***  This field, if present, indicates that the target device supports the *NR-DL-PRS-ExpectedLOS-NLOS-Assistance* in IE *NR-PositionCalculationAssistance*:  - *type* indicates whether the target device supports '*hard*' value or '*hard*' and '*soft*' value in *LOS-NLOS-Indicator* in IE *NR-DL-PRS-ExpectedLOS-NLOS-Assistance*.  - *granularity* indicates whether the target device supports *nr-los-nlos-indicator* in IE *NR-DL-PRS-ExpectedLOS-NLOS-Assistance* '*per-trp*', '*per-resource*', or both.  The UE can include this field only if the UE supports one of *maxDL-PRS-RSRP-MeasurementFR1*, *maxDL-PRS-RSRP-MeasurementFR2*, *dl-RSTD-MeasurementPerPairOfTRP-FR1*, *dl-RSTD-MeasurementPerPairOfTRP-FR*2, *maxNrOfRx-TX-MeasFR1*, *maxNrOfRx-TX-MeasFR2*, *supportOfRSRP-MeasFR1* and *supportOfRSRP-MeasFR2*. Otherwise, the UE does not include this field. |
| ***nr-DL-PRS-ExpectedAoD-or-AoA-Sup***  This field, if present, indicates that the target device supports the *NR-DL-PRS-ExpectedAoD-or-AoA* in *NR-DL-PRS-AssistanceData.* |
| ***nr-DL-TDOA-On-Demand-DL-PRS-Support***  This field, if present, indicates that the target device supports on-demand DL-PRS requests. |
| ***nr-los-nlos-IndicatorSupport***  This field, if present, indicates that the target device supports *nr-los-nlos-Indicator* reporting in IE *NR-DL-TDOA-SignalMeasurementInformation*.  - *type* indicates whether the target device supports '*hard*' value or '*hard*' and '*soft*' value in IE *LOS-NLOS-Indicator.*  - *granularity* indicates whether the target device supports *LOS-NLOS-Indicator* reporting per TRP, per DL-PRS Resource, or both.  NOTE: A single value is reported when both Multi-RTT and DL-TDOA are supported. |
| ***additionalPathsExtSupport***  This field, if present, indicates that the target device supports the *nr-AdditionalPathListExt* reporting in IE *NR-DL-TDOA-SignalMeasurementInformation*. The enumerated value indicates the number of additional paths supported by the target device.  NOTE: The *supportOfDL-PRS-FirstPathRSRP* in IE *NR-DL-TDOA-MeasurementCapability* also applies to the additional paths. |
| ***scheduledLocationRequestSupported***  This field, if present, specifies the positioning modes for which the target device supports scheduled location requests – i.e., supports the IE *ScheduledLocationTime* in IE *CommonIEsRequestLocationInformation* – and the time base(s) supported for the scheduled location time for each positioning mode. If this field is absent, the target device does not support scheduled location requests. |
| ***nr-dl-prs-AssistanceDataValidity***  This field, if present, indicates that the target device supports validity conditions for pre-configured assistance data and comprises the following subfields:  - ***area-validity*** indicates that the target device supports pre-configured assistance data with area validity. The integer number indicates the maximum number of areas the target device supports*.* |
| ***multiMeasInSameMeasReport***  This field, if present, indicates that the target device supports multiple measurement instances in a single measurement report. |
| ***mg-ActivationRequest***  This field, if present, indicates that the target device supports UL MAC CE for positioning measurement gap activation/deactivation request for DL-PRS measurements. The UE can include this field only if the UE supports *mg-ActivationRequestPRS-Meas* and *mg-ActivationCommPRS-Meas* defined in TS 38.331 [35]. |
| ***posMeasGapSupport***  This field, if present, indicates that the target device supports pre-configured positioning measurement gap for DL-PRS measurements. The UE can include this field only if the UE supports *mg-ActivationCommPRS-Meas* defined in TS 38.331 [35]. |
| ***multiLocationEstimateInSameMeasReport***  This field, if present, indicates that the target device supports multiple location estimate instances in a single measurement report. |
| ***locationCoordinateTypes***  This field indicates the geographical location coordinate types that a target device supports for UE-based DL-TDOA. TRUE indicates that a location coordinate type is supported and FALSE that it is not. |
| ***periodicAssistanceData***  This field identifies the periodic NR assistance data delivery procedures supported by the target device. This is represented by a bit string, with a one value at the bit position means the periodic NR assistance data delivery procedure is supported; a zero value means not supported. Bit 0 (solicited) represents the procedure according to clause 5.2.1a; bit (1) (unsolicited) represents the procedure according to clause 5.2.2a. |
| ***nr-IntegrityAssistanceSupport***  This field indicates the Integrity Assistance Data supported. This is represented by a bit string, with a one‑value at the bit position means the particular assistance data is supported; a zero‑value means not supported.  - bit 0 indicates whether the field *nr-IntegrityServiceParameters* in IE *NR-PositionCalculationAssistance* is supported or not;  - bit 1 indicates whether the field *nr-IntegrityServiceAlert* in IE *NR-PositionCalculationAssistance* is supported or not;  - bit 2 indicates whether the field *nr-IntegrityRiskParameters* in IE *NR-PositionCalculationAssistance* is supported or not;  - bit 3 indicates whether the field *nr-IntegrityParametersTRP-LocationInfo* in IE *NR-PositionCalculationAssistance* is supported or not;  - bit 4 indicates whether the field *nr-IntegrityParametersDL-PRS-BeamInfo* in IE *NR-PositionCalculationAssistance* is supported or not;  - bit 5 indicates whether the field *nr-IntegrityParametersRTD-Info* in IE *NR-PositionCalculationAssistance* is supported or not. |
| ***nr-DL-TDOA-OnDemandPRS-ForBWA-Support***  This field, if present, indicates that the target device supports on-demand DL-PRS request for bandwidth aggregation. |
| ***periodicReportingIntervalMsSupport***  This field, if present, specified the supported minimum millisecond periodic reporting interval for location information per positioning mode – i.e., supports the subfield *reportingIntervalMs* of the IE *PeriodicalReportingCriteriaExt* in IE *CommonIEsRequestLocationInformation* – and the minimum millisecond report interval supported for the periodic reporting. |

#### 6.5.10.6a NR DL-TDOA Capability Information Elements

#### *– NR-DL-TDOA-MeasurementCapability*

The IE *NR-DL-TDOA-MeasurementCapability* defines the DL-TDOA measurement capability. The UE can include this IE only if the UE supports *NR-DL-PRS-ResourcesCapability* for DL-TDOA. Otherwise, the UE does not include this IE.

-- ASN1START

NR-DL-TDOA-MeasurementCapability-r16 ::= SEQUENCE {

dl-RSTD-MeasurementPerPairOfTRP-FR1-r16 INTEGER (1..4),

dl-RSTD-MeasurementPerPairOfTRP-FR2-r16 INTEGER (1..4),

supportOfDL-PRS-RSRP-MeasFR1-r16 ENUMERATED { supported} OPTIONAL,

supportOfDL-PRS-RSRP-MeasFR2-r16 ENUMERATED { supported} OPTIONAL,

...,

[[

nr-UE-TEG-Capability-r17 NR-UE-TEG-Capability-r17 OPTIONAL,

dl-tdoa-MeasCapabilityBandList-r17 SEQUENCE (SIZE (1..nrMaxBands-r16)) OF

DL-TDOA-MeasCapabilityPerBand-r17 OPTIONAL

]]

}

DL-TDOA-MeasCapabilityPerBand-r17 ::= SEQUENCE {

freqBandIndicatorNR-r17 FreqBandIndicatorNR-r16,

supportOfDL-PRS-FirstPathRSRP-r17 ENUMERATED { supported } OPTIONAL,

dl-PRS-MeasRRC-Inactive-r17 ENUMERATED { supported } OPTIONAL,

...,

[[

supportOfDL-PRS-BWA-RRC-Connected-r18 ENUMERATED { supported } OPTIONAL,

supportOfDL-PRS-BWA-RRC-Inactive-r18 ENUMERATED { supported } OPTIONAL,

supportOfDL-PRS-BWA-RRC-Idle-r18 ENUMERATED { supported } OPTIONAL,

nr-DL-PRS-RSCPD-RRC-Connected-r18 ENUMERATED { supported } OPTIONAL,

assocSingleRSTD-WithUpToNsampleRSCPD-r18 ENUMERATED { supported } OPTIONAL,

nr-DL-PRS-RSCPD-MeasurementRRC-Idle-r18 ENUMERATED { supported } OPTIONAL,

supportOfUE-basedCarrierPhasePositioning-r18 ENUMERATED { supported } OPTIONAL,

supportOfSymbolTimeStampForRSCPD-r18 ENUMERATED { supported } OPTIONAL,

supportOfFinerTimingReportGranularityForPRS-Meas-r18 ENUMERATED { minus1, minus2,

minus3, minus4, minus5, minus6}

OPTIONAL,

supportOfMeasurementsInTimeWindow-r18 BIT STRING { rstd (0),

rsrp (1),

rsrpp (2),

rscpd (3)

} (SIZE (1..8)) OPTIONAL,

supportOfPRS-MeasurementRRC-Idle-r18 ENUMERATED { supported } OPTIONAL

]],

[[

nr-DL-PRS-RSCPD-RRC-Inactive-r18 ENUMERATED { supported } OPTIONAL

]]

}

-- ASN1STOP

|  |
| --- |
| *NR-DL-TDOA-MeasurementCapability* field descriptions |
| ***dl-RSTD-MeasurementPerPairOfTRP-FR1***  Indicates number of DL RSTD measurements per pair of TRPs on FR1. |
| ***dl-RSTD-MeasurementPerPairOfTRP-FR2***  Indicates number of DL RSTD measurements per pair of TRPs on FR2. |
| ***supportOfDL-PRS-RSRP-MeasFR1***  Indicates whether the UE supports DL-PRS RSRP measurement for DL-TDOA on FR1. |
| ***supportOfDL-PRS-RSRP-MeasFR2***  Indicates whether the UE supports DL-PRS RSRP measurement for DL-TDOA on FR2. |
| ***nr-UE-TEG-Capability***  Indicates the UE TEG capability. |
| ***supportOfDL-PRS-FirstPathRSRP***  Indicates whether the target device supports DL-PRS RSRPP of first path measurement for DL-TDOA. The UE can include this field only if the UE supports *prs-ProcessingCapabilityBandList*. Otherwise, the UE does not include this field. The UE supporting *additionalPathsReport* and *supportOfDL-PRS-FirstPathRSRP* shall support RSRPP reporting for K=1 or 2 additional paths. |
| ***dl-PRS-MeasRRC-Inactive***  This field, if present, indicates that the target device supports DL-PRS measurement in RRC\_INACTIVE state. The UE can include this field only if the UE supports *maxNrOfDL-PRS-ResourceSetPerTrpPerFrequencyLayer, maxNrOfTRP-AcrossFreqs, maxNrOfPosLayer* and *dl-PRS-BufferType-RRC-Inactive*. Otherwise, the UE does not include this field.  NOTE 1: This capability is applicable to both, UE-assisted and UE-based DL-TDOA.  NOTE 2: The capabilities *NR-DL-PRS-ResourcesCapability, dl-RSTD-MeasurementPerPairOfTRP-FR1, dl-RSTD-MeasurementPerPairOfTRP-FR2, supportOfDL-PRS-RSRP-MeasFR1, supportOfDL-PRS-RSRP-MeasFR2, simul-NR-DL-AoD-DL-TDOA* are the same in RRC\_INACTIVE state. |
| ***supportOfDL-PRS-BWA-RRC-Connected***  Indicates whether the target device supports DL-PRS bandwidth aggregation in RRC\_CONNECTED for DL-TDOA.  The UE can include this field only if the UE supports *maxNrOfDL-PRS-ResourceSetPerTrpPerFrequencyLayer, maxNrOfTRP-AcrossFreqs, maxNrOfPosLayer* and *prs-BWA-TwoContiguousIntrabandInMG-RRC-Connected*. Otherwise, the UE does not include this field. |
| ***supportOfDL-PRS-BWA-RRC-Inactive***  Indicates whether the target device supports DL-PRS bandwidth aggregation in RRC\_INACTIVE for DL-TDOA.  The UE can include this field only if the UE supports *dl-PRS-MeasRRC-Inactive* and *prs-BWA-TwoContiguousIntraband-RRC-IdleAndInactive*. Otherwise, the UE does not include this field. |
| ***supportOfDL-PRS-BWA-RRC-Idle***  Indicates whether the target device supports DL-PRS bandwidth aggregation in RRC\_IDLE for DL-TDOA.  The UE can include this field only if the UE supports *supportOfPRS-MeasurementRRC-Idle* and *prs-BWA-TwoContiguousIntraband-RRC-IdleAndInactive*. Otherwise, the UE does not include this field. |
| ***nr-DL-PRS-RSCPD-RRC-Connected***  This field, if present, indicates that the target device supports DL RSCPD measurements in RRC\_CONNECTED.  The UE can include this field only if the UE supports *dl-RSTD-MeasurementPerPairOfTRP-FR1* and *dl-RSTD-MeasurementPerPairOfTRP-FR2*. Otherwise, the UE does not include this field.  NOTE 3: RSCPD is reported together with RSTD measurement. |
| ***assocSingleRSTD-WithUpToNsampleRSCPD***  This field, if present, indicates that the target device supports associating a single RSTD measurement with up to N\_sample RSCPD measurement. The UE can include this field only if the UE supports one of *nr-DL-PRS-RSCPD-RRC-Connected* and *nr-DL-PRS-RSCPD-RRC-Inactive*. Otherwise, the UE does not include this field. |
| ***nr-DL-PRS-RSCPD-MeasurementRRC-Idle***  This field, if present, indicates that the target device supports DL RSCPD measurement based on DL-PRS measurement in RRC\_IDLE. The UE can include this field only if the UE supports *supportOfPRS-MeasurementRRC-Idle*. Otherwise, the UE does not include this field.  NOTE 5: DL RSCPD is reported along with measurement report for DL-RSTD |
| ***supportOfUE-basedCarrierPhasePositioning***  This field, if present, indicates that the target device supports carrier phase measurement for UE-based positioning and support of assistance data for UE-based carrier phase positioning. |
| ***supportOfSymbolTimeStampForRSCPD***  This field, if present, indicates that the target device supports reporting timestamp with OFDM symbol index associated with RSCPD measurement. The UE can include this field only if the UE supports one of *nr-DL-PRS-RSCPD-RRC-Connected* and *nr-DL-PRS-RSCPD-RRC-Inactive*. Otherwise, the UE does not include this field. |
| ***supportOfFinerTimingReportGranularityForPRS-Meas***  This field, if present, indicates that the target device supports of finer timing reporting granularity for DL-PRS measurement. |
| ***supportOfMeasurementsInTimeWindow***  This field, if present, indicates that the target device supports performing measurements inside the indicated time window only for DL-TDOA. This is represented by a bit string, with a one‑value at the bit position means the particular measurement is supported; a zero‑value means not supported.  - bit 0 indicates whether performing DL RSTD is supported or not;  - bit 1 indicates whether performing DL PRS-RSRP is supported or not;  - bit 2 indicates whether performing DL PRS-RSRPP is supported or not;  - bit 3 indicates whether performing DL PRS-RSCPD is supported or not;  The UE can include this field only if the UE supports *maxNrOfDL-PRS-ResourcesPerResourceSet* and *maxNrOfDL-PRS-ResourcesPerPositioningFrequencylayer*. Otherwise, the UE does not include this field. |
| ***supportOfPRS-MeasurementRRC-Idle***  Indicates whether the UE supports DL-PRS measurement in RRC\_IDLE for DL-TDOA. The UE can include this field only if the UE supports *supportedBandwidthPRS, dl-PRS-BufferType, durationOfPRS-Processing, maxNumOfDL-PRS-ResProcessedPerSlot,* *dl-PRS-BufferType-RRC-Inactive, durationOfPRS-Processing-RRC-Inactive, maxNumOfDL-PRS-ResProcessedPerSlot-RRC-Inactive* and *dl-PRS-MeasRRC-Inactive*. Otherwise, the UE does not include this field. |
| ***nr-DL-PRS-RSCPD-RRC-Inactive***  This field, if present, indicates that the target device supports DL RSCPD measurements in RRC\_INACTIVE. The UE can include this field only if the UE supports *dl-PRS-MeasRRC-Inactive*. Otherwise, the UE does not include this field.  NOTE 4: RSCPD is reported together with RSTD measurement. |

#### 6.5.10.7 NR DL-TDOA Capability Information Request

#### – *NR-DL-TDOA-RequestCapabilities*

The IE *NR-DL-TDOA-RequestCapabilities* is used by the location server to request the capability of the target device to support NR DL-TDOA and to request NR DL-TDOA positioning capabilities from a target device.

-- ASN1START

NR-DL-TDOA-RequestCapabilities-r16 ::= SEQUENCE {

...

}

-- ASN1STOP

#### 6.5.10.8 NR DL-TDOA Error Elements

#### – *NR-DL-TDOA-Error*

The IE *NR-DL-TDOA-Error* is used by the location server or target device to provide NR DL-TDOA error reasons to the target device or location server, respectively.

-- ASN1START

NR-DL-TDOA-Error-r16 ::= CHOICE {

locationServerErrorCauses-r16 NR-DL-TDOA-LocationServerErrorCauses-r16,

targetDeviceErrorCauses-r16 NR-DL-TDOA-TargetDeviceErrorCauses-r16,

...

}

-- ASN1STOP

#### – *NR-DL-TDOA-LocationServerErrorCauses*

The IE *NR-DL-TDOA-LocationServerErrorCauses* is used by the location server to provide NR DL-TDOA error reasons to the target device.

-- ASN1START

NR-DL-TDOA-LocationServerErrorCauses-r16 ::= SEQUENCE {

cause-r16 ENUMERATED { undefined,

assistanceDataNotSupportedByServer,

assistanceDataSupportedButCurrentlyNotAvailableByServer,

notProvidedAssistanceDataNotSupportedByServer,

...,

on-demand-dl-prs-NotSupportedByServer-v1700,

on-demand-dl-prs-SupportedButCurrentlyNotAvailableByServer-v1700

},

...

}

-- ASN1STOP

#### – *NR-DL-TDOA-TargetDeviceErrorCauses*

The IE *NR-DL-TDOA-TargetDeviceErrorCauses* is used by the target device to provide NR DL-TDOA error reasons to the location server.

-- ASN1START

NR-DL-TDOA-TargetDeviceErrorCauses-r16 ::= SEQUENCE {

cause-r16 ENUMERATED { undefined,

assistance-data-missing,

unableToMeasureAnyTRP,

attemptedButUnableToMeasureSomeNeighbourTRPs,

thereWereNotEnoughSignalsReceivedForUeBasedDL-TDOA,

locationCalculationAssistanceDataMissing,

...

},

...,

[[

remoteUE-Indication-r18 ENUMERATED {true} OPTIONAL -- Cond NR

]]

}

-- ASN1STOP

| Conditional presence | Explanation |
| --- | --- |
| *NR* | This field is optionally present, need OR, for NR access. Otherwise it is not present. |

| *NR-DL-TDOA-TargetDeviceErrorCauses* field descriptions |
| --- |
| ***remoteUE-Indication***  This field indicates whether the target device in NR access is configured as a L2 U2N Remote UE. |

### 6.5.11 NR DL-AoD Positioning

This clause defines the information elements for NR downlink AoD positioning (TS 38.305 [40]).

#### 6.5.11.1 NR DL-AoD Assistance Data

#### – *NR-DL-AoD-ProvideAssistanceData*

The IE *NR-DL-AoD-ProvideAssistanceData* is used by the location server to provide assistance data to enable UE‑assisted and UE-based NR DL-AoD. It may also be used to provide NR DL-AoD positioning specific error reason.

-- ASN1START

NR-DL-AoD-ProvideAssistanceData-r16 ::= SEQUENCE {

nr-DL-PRS-AssistanceData-r16 NR-DL-PRS-AssistanceData-r16 OPTIONAL, -- Need ON

nr-SelectedDL-PRS-IndexList-r16 NR-SelectedDL-PRS-IndexList-r16 OPTIONAL, -- Need ON

nr-PositionCalculationAssistance-r16

NR-PositionCalculationAssistance-r16

OPTIONAL, -- Cond UEB

nr-DL-AoD-Error-r16 NR-DL-AoD-Error-r16 OPTIONAL, -- Need ON

...,

[[

nr-DL-PRS-BeamInfo-r17 NR-DL-PRS-BeamInfo-r16 OPTIONAL, -- Cond UEA

nr-On-Demand-DL-PRS-Configurations-r17

NR-On-Demand-DL-PRS-Configurations-r17

OPTIONAL, -- Need ON

nr-On-Demand-DL-PRS-Configurations-Selected-IndexList-r17

NR-On-Demand-DL-PRS-Configurations-Selected-IndexList-r17

OPTIONAL, -- Need ON

assistanceDataValidityArea-r17 AreaID-CellList-r17 OPTIONAL -- Need ON

]]

}

-- ASN1STOP

| Conditional presence | Explanation |
| --- | --- |
| *UEB* | The field is optionally present, need ON, for UE based NR DL-AoD; otherwise it is not present. |
| *UEA* | The field is optionally present, need ON, for UE-assisted NR DL-AoD; otherwise it is not present. |

|  |
| --- |
| *NR-DL-AoD-ProvideAssistanceData* field descriptions |
| ***nr-DL-PRS-AssistanceData***  This field specifies the assistance data reference and neighbour TRPs and provides the DL-PRS configuration for the TRPs.  Note, if this field is absent but the *nr-SelectedDL-PRS-IndexList* field is present, the *nr-DL-PRS-AssistanceData* may be provided in IE *NR-Multi-RTT-ProvideAssistanceData*, *NR-DL-TDOA-ProvideAssistanceData*, or *NR-AI-ML-PositioningProvideAssistanceData*. |
| ***nr-SelectedDL-PRS-IndexList***  This field specifies the DL-PRS Resources which are applicable for this *NR-DL-AoD-ProvideAssistanceData* message. |
| ***nr-PositionCalculationAssistance***  This field provides position calculation assistance data for UE-based mode. |
| ***nr-DL-AoD-Error***  This field provides DL-AoD error reasons. |
| ***nr-DL-PRS-BeamInfo***  This field provides spatial direction information of the DL-PRS Resources included in *nr-DL-PRS-AssistanceData* or indicated by *nr-SelectedDL-PRS-IndexList.* |
| ***nr-On-Demand-DL-PRS-Configurations***  This field provides a set of available DL-PRS configurations which can be requested by the target device on-demand.  NOTE 1: Void.  NOTE 2: If this field is absent but the *nr-On-Demand-DL-PRS-Configurations-Selected-IndexList* is present, the *nr-On-Demand-DL-PRS-Configurations* may be provided in IE *NR-Multi-RTT-ProvideAssistanceData* *NR-DL-TDOA-ProvideAssistanceData*, or *NR-AI-ML-PositioningProvideAssistanceData*. |
| ***nr-On-Demand-DL-PRS-Configurations-Selected-IndexList***  This field specifies the selected available on-demand DL-PRS configurations which are applicable for this *NR-DL-AoD-ProvideAssistanceData message*. |
| ***assistanceDataValidityArea***  This field specifies the network area for which this *NR-DL-AoD-ProvideAssistanceData* is valid. |

Editor's Note: It is FFS whether DL-PRS and on-demand PRS assistance data are applicable to AI/ML positioning.

#### 6.5.11.2 NR DL-AoD Assistance Data Request

#### – *NR-DL-AoD-RequestAssistanceData*

The IE *NR-DL-AoD-RequestAssistanceData* is used by the target device to request assistance data from a location server.

-- ASN1START

NR-DL-AoD-RequestAssistanceData-r16 ::= SEQUENCE {

nr-PhysCellID-r16 NR-PhysCellID-r16 OPTIONAL,

nr-AdType-r16 BIT STRING { dl-prs (0),

posCalc (1) } (SIZE (1..8)),

...,

[[

nr-PosCalcAssistanceRequest-r17 BIT STRING { trpLoc (0),

beamInfo (1),

rtdInfo (2),

beamAntInfo (3),

losNlosInfo (4),

nr-IntegrityBounds-r18 (5)

} (SIZE (1..8)) OPTIONAL,

nr-DL-PRS-ExpectedAoD-or-AoA-Request-r17 ENUMERATED { eAoD, eAoA } OPTIONAL,

nr-DL-PRS-BeamInfoRequest-r17 ENUMERATED { requested } OPTIONAL,

nr-on-demand-DL-PRS-Request-r17 NR-On-Demand-DL-PRS-Request-r17 OPTIONAL,

pre-configured-AssistanceDataRequest-r17 ENUMERATED { true } OPTIONAL,

nr-IntegrityAssistanceRequest-r18 BIT STRING {

serviceParameters (0),

serviceAlert (1),

riskParameters (2),

integrityParaTRP-Loc (3),

integrityParaBeamInfo (4),

integrityParaRTD-Info (5),

integrityBeamAntInfo (6)

} (SIZE (1..8)) OPTIONAL

]]

}

-- ASN1STOP

|  |
| --- |
| *NR-DL-AoD-RequestAssistanceData* field descriptions |
| ***nr-PhysCellID***  This field specifies the NR physical cell identity of the current primary cell of the target device. |
| ***nr-AdType***  This field indicates the requested assistance data. *dl-prs* means requested assistance data is *nr-DL-PRS-AssistanceData*, *posCalc* means requested assistance data is *nr-PositionCalculationAssistance* for UE based positioning. |
| ***nr-PosCalcAssistanceRequest***  This field indicates the Position Calculation Assistance Data requested. This is represented by a bit string, with a one‑value at the bit position means the particular assistance data is requested; a zero‑value means not requested.  - bit 0 indicates whether the field *nr-TRP-LocationInfo* in IE *NR-PositionCalculationAssistance* is requested or not;  - bit 1 indicates whether the field *nr-DL-PRS-BeamInfo* in IE *NR-PositionCalculationAssistance* is requested or not;  - bit 2 indicates whether the field *nr-RTD-Info* in IE *NR-PositionCalculationAssistance* is requested or not;  - bit 3 indicates whether the field *nr-TRP-BeamAntennaInfo* in IE *NR-PositionCalculationAssistance* is requested or not;  - bit 4 indicates whether the field *nr-DL-PRS-Expected-LOS-NLOS-Assistance* in IE *NR-PositionCalculationAssistance* is requested or not;  - bit 5 together with bit 0 indicates whether the fields *nr-IntegrityTRP-LocationBounds*, *nr-IntegrityDL-PRS-ResourceSetARP-LocationBounds*, *nr-IntegrityDL-PRS-ResourceARP-LocationBounds* in IE *NR-TRP-LocationInfo* are requested or not; bit 5 together with bit 1 indicates whether the field *nr-IntegrityBeamInfoBounds* in IE *NR-DL-PRS-BeamInfo* is requested or not; bit 5 together with bit 2 indicates whether the field *nr-IntegrityRTD-InfoBounds* in IE *NR-RTD-Info* is requested or not; bit 5 together with bit 3 indicates whether the field *nr-integrityBeamPowerBounds* in IE *NR-TRP-BeamAntennaInfo* is requested or not.  This field may only be present if the '*posCalc*' bit in *nr-AdType* is set to value '1'. |
| ***nr-DL-PRS-ExpectedAoD-or-AoA-Request***  This field, if present, indicates that the IE *NR-DL-PRS-ExpectedAoD-or-AoA* in *NR-DL-PRS-AssistanceData* is requested. Enumerated value '*eAoD*' indicates that expected AoD information is requested; value 'eAoA' indicates that expected AoA information is requested.  This field may only be present if the '*dl-prs*' bit in *nr-AdType* is set to value '1'. |
| ***nr-DL-PRS-BeamInfoRequest***  This field, if present, indicates that the IE *NR-DL-PRS-BeamInfo* is requested. |
| ***nr-on-demand-DL-PRS-Request***  This field indicates the on-demand DL-PRS requested for DL-AoD. This field may be included when the *dl-prs* bit in *nr-AdType* is set to value '1'. |
| ***pre-configured-AssistanceDataRequest***  This field, if present, indicates that the target device requests pre-configured assistance data with area validity. |
| ***nr-IntegrityAssistanceRequest***  This field indicates the Integrity Assistance Data requested. This is represented by a bit string, with a one‑value at the bit position means the particular assistance data is requested; a zero‑value means not requested.  - bit 0 indicates whether the field *nr-IntegrityServiceParameters* in IE *NR-PositionCalculationAssistance* is requested or not;  - bit 1 indicates whether the field *nr-IntegrityServiceAlert* in IE *NR-PositionCalculationAssistance* is requested or not;  - bit 2 indicates whether the field *nr-IntegrityRiskParameters* in IE *NR-PositionCalculationAssistance* is requested or not;  - bit 3 indicates whether the field *nr-IntegrityParametersTRP-LocationInfo* in IE *NR-PositionCalculationAssistance* is requested or not;  - bit 4 indicates whether the field *nr-IntegrityParametersDL-PRS-BeamInfo* in IE *NR-PositionCalculationAssistance* is requested or not;  - bit 5 indicates whether the field *nr-IntegrityParametersRTD-Info* in IE *NR-PositionCalculationAssistance* is requested or not;  - bit 6 indicates whether the field *nr-IntegrityParametersTRP-BeamAntennaInfo* in IE *NR-PositionCalculationAssistance* is requested or not. |

#### 6.5.11.3 NR DL-AoD Location Information

#### – *NR-DL-AoD-ProvideLocationInformation*

The IE *NR-DL-AoD-ProvideLocationInformation* is used by the target device to provide NR DL-AoD location measurements to the location server. It may also be used to provide NR DL-AoD positioning specific error reason.

-- ASN1START

NR-DL-AoD-ProvideLocationInformation-r16 ::= SEQUENCE {

nr-DL-AoD-SignalMeasurementInformation-r16

NR-DL-AoD-SignalMeasurementInformation-r16

OPTIONAL,

nr-dl-AoD-LocationInformation-r16 NR-DL-AoD-LocationInformation-r16

OPTIONAL,

nr-DL-AoD-Error-r16 NR-DL-AoD-Error-r16 OPTIONAL,

...,

[[

nr-DL-AoD-SignalMeasurementInstances-r17 SEQUENCE (SIZE (1..maxMeasInstances-r17)) OF

NR-DL-AoD-SignalMeasurementInformation-r16 OPTIONAL, -- Cond batchUEA

nr-DL-AoD-LocationInformationInstances-r17 SEQUENCE (SIZE (1..maxMeasInstances-r17)) OF

NR-DL-AoD-LocationInformation-r16 OPTIONAL -- Cond batchUEB

]]

}

-- ASN1STOP

| Conditional presence | Explanation |
| --- | --- |
| *batchUEA* | The field is optionally present if the field *nr-DL-AoD-SignalMeasurementInformation* is absent; otherwise it is not present. |
| *batchUEB* | The field is optionally present if the field *nr-dl-AoD-LocationInformation* is absent; otherwise it is not present. |

#### 6.5.11.4 NR DL-AoD Location Information Elements

#### – *NR-DL-AoD-SignalMeasurementInformation*

The IE *NR-DL-AoD-SignalMeasurementInformation* is used by the target device to provide NR DL-AoD measurements to the location server.

-- ASN1START

NR-DL-AoD-SignalMeasurementInformation-r16 ::= SEQUENCE {

nr-DL-AoD-MeasList-r16 NR-DL-AoD-MeasList-r16,

...

}

NR-DL-AoD-MeasList-r16 ::= SEQUENCE (SIZE(1..nrMaxTRPs-r16)) OF NR-DL-AoD-MeasElement-r16

NR-DL-AoD-MeasElement-r16 ::= SEQUENCE {

dl-PRS-ID-r16 INTEGER (0..255),

nr-PhysCellID-r16 NR-PhysCellID-r16 OPTIONAL,

nr-CellGlobalID-r16 NCGI-r15 OPTIONAL,

nr-ARFCN-r16 ARFCN-ValueNR-r15 OPTIONAL,

nr-DL-PRS-ResourceID-r16 NR-DL-PRS-ResourceID-r16 OPTIONAL,

nr-DL-PRS-ResourceSetID-r16 NR-DL-PRS-ResourceSetID-r16 OPTIONAL,

nr-TimeStamp-r16 NR-TimeStamp-r16,

nr-DL-PRS-RSRP-Result-r16 INTEGER (0..126),

nr-DL-PRS-RxBeamIndex-r16 INTEGER (1..8) OPTIONAL,

nr-DL-AoD-AdditionalMeasurements-r16

NR-DL-AoD-AdditionalMeasurements-r16 OPTIONAL,

...,

[[

nr-DL-PRS-FirstPathRSRP-Result-r17

INTEGER (0..126) OPTIONAL,

nr-los-nlos-Indicator-r17 CHOICE {

perTRP-r17 LOS-NLOS-Indicator-r17,

perResource-r17 LOS-NLOS-Indicator-r17

} OPTIONAL,

nr-DL-AoD-AdditionalMeasurementsExt-r17

NR-DL-AoD-AdditionalMeasurementsExt-r17 OPTIONAL

]],

[[

nr-ReportDL-PRS-MeasBasedOnSingleOrMultiHopRx-r18

ENUMERATED { singleHop, multipleHop } OPTIONAL

]]

}

NR-DL-AoD-AdditionalMeasurements-r16 ::= SEQUENCE (SIZE (1..7)) OF

NR-DL-AoD-AdditionalMeasurementElement-r16

NR-DL-AoD-AdditionalMeasurementsExt-r17 ::= SEQUENCE (SIZE (1..maxAddMeasAoD-r17)) OF

NR-DL-AoD-AdditionalMeasurementElement-r17

NR-DL-AoD-AdditionalMeasurementElement-r16 ::= SEQUENCE {

nr-DL-PRS-ResourceID-r16 NR-DL-PRS-ResourceID-r16 OPTIONAL,

nr-DL-PRS-ResourceSetID-r16 NR-DL-PRS-ResourceSetID-r16 OPTIONAL,

nr-TimeStamp-r16 NR-TimeStamp-r16,

nr-DL-PRS-RSRP-ResultDiff-r16 INTEGER (0..30),

nr-DL-PRS-RxBeamIndex-r16 INTEGER (1..8) OPTIONAL,

...

}

NR-DL-AoD-AdditionalMeasurementElement-r17 ::= SEQUENCE {

nr-DL-PRS-ResourceID-r17 NR-DL-PRS-ResourceID-r16 OPTIONAL,

nr-DL-PRS-ResourceSetID-r17 NR-DL-PRS-ResourceSetID-r16 OPTIONAL,

nr-TimeStamp-r17 NR-TimeStamp-r16,

nr-DL-PRS-RSRP-ResultDiff-r17 INTEGER (0..30) OPTIONAL, -- Cond rsrp

nr-DL-PRS-RxBeamIndex-r17 INTEGER (1..8) OPTIONAL,

nr-DL-PRS-FirstPathRSRP-ResultDiff-r17 INTEGER (0..61) OPTIONAL, -- Cond rsrpp

nr-los-nlos-IndicatorPerResource-r17 LOS-NLOS-Indicator-r17 OPTIONAL,

...,

[[

nr-ReportDL-PRS-MeasBasedOnSingleOrMultiHopRx-r18

ENUMERATED { singleHop, multipleHop } OPTIONAL

]]

}

-- ASN1STOP

| Conditional presence | Explanation |
| --- | --- |
| *rsrp* | The field is mandatory present if the field *nr-DL-PRS-FirstPathRSRP-ResultDiff-r17* is absent; otherwise it is optionally present, need ON. |
| *rsrpp* | The field is mandatory present if the field *nr-DL-PRS-RSRP-ResultDiff-r17* is absent; otherwise it is optionally present, need ON. |

|  |
| --- |
| *NR-DL-AoD-SignalMeasurementInformation* field descriptions |
| ***dl-PRS-ID***  This field is used along with a DL-PRS Resource Set ID and a DL-PRS Resource ID to uniquely identify a DL-PRS Resource. This ID can be associated with multiple DL-PRS Resource Sets associated with a single TRP.  Each TRP should only be associated with one such ID. |
| ***nr-PhysCellID***  This field specifies the physical cell identity of the associated TRP, as defined in TS 38.331 [35]. |
| ***nr-CellGlobalID***  This field specifies the NCGI, the globally unique identity of a cell in NR, of the associated TRP, as defined in TS 38.331 [35]. |
| ***nr-ARFCN***  This field specifies the NR-ARFCN of the TRP's CD-SSB (as defined in TS 38.300 [47]) corresponding to *nr-PhysCellID*. |
| ***nr-TimeStamp***  This field specifies the time instance at which the measurement is performed. |
| ***nr-DL-PRS-RSRP-Result***  This field specifies the NR DL-PRS reference signal received power (DL-PRS RSRP) measurement, as defined in TS 38.215 [36]. The mapping of the measured quantity is defined as in TS 38.133 [46]. |
| ***nr-DL-PRS-RxBeamIndex***  This field provides an index of the target device receive beam used for DL-PRS measurements associated with a single TRP in *nr-DL-AoD-MeasList-r16* when additional DL-PRS measurements are also included in either *nr-DL-AoD-AdditionalMeasurements-r16* or *nr-DL-AoD-AdditionalMeasurementsExt-r17*. If the value of the receive beam index for two or more DL-PRS measurements is the same, it indicates that the target device receive beam for the two or more DL-PRS measurements associated with a TRP were made with the same RX beam. The field is mandatory present if at least two DL-PRS RSRP measurements and/or DL-PRS RSRPP measurements from the same DL-PRS Resource Set associated with a TRP have been made with the same RX beam by the target device; otherwise it is not present. |
| ***nr-DL-AoD-AdditionalMeasurements***  This field specifies a list of additional DL-PRS RSRP measurements of different DL-PRS resources for the same TRP. If this field is present, the field *nr-DL-AoD-AdditionalMeasurementsExt* should not be present. |
| ***nr-DL-PRS-FirstPathRSRP-Result***  This field specifies the NR DL-PRS reference signal received path power (DL-PRS RSRPP) of the first detected path in time, as defined in TS 38.215 [36]. The mapping of the measured quantity is defined as in TS 38.133 [46]. |
| ***nr-los-nlos-Indicator***  This field specifies the target device's best estimate of the LOS or NLOS of the RSRP or RSRPP of first path measurement for the TRP or resource.  NOTE: If the requested type or granularity in *nr-los-nlos-IndicatorRequest* is not possible, the target device may provide a different type and granularity for the estimated *LOS-NLOS-Indicator.* |
| ***nr-DL-AoD-AdditionalMeasurementsExt***  This field specifies a list of additional DL-PRS RSRP and/or DL-PRS RSRPP measurements of different DL-PRS resources for the same TRP. If this field is present, the field *nr-DL-AoD-AdditionalMeasurements* should not be present. |
| ***nr-DL-PRS-RSRP-ResultDiff***  This field provides the additional DL-PRS RSRP measurement result relative to *nr-DL-PRS-RSRP-Result*. The DL-PRS RSRP value of this measurement is obtained by adding the value of this field to the value of the *nr-DL-PRS-RSRP-Result* field. The mapping of the field is defined in TS 38.133 [46]. |
| ***nr-DL-PRS-FirstPathRSRP-ResultDiff***  This field specifies the additional NR DL-PRS reference signal received path power (DL-PRS RSRPP) of the first detected path in time relative to *nr-DL-PRS-FirstPathRSRP-Result*. The DL-PRS RSRPP of first path value of this measurement is obtained by adding the value of this field to the value of the *nr-DL-PRS-FirstPathRSRP-Result* field. The mapping of the field is defined in TS 38.133 [46]. |
| ***nr-los-nlos-IndicatorPerResource***  This field specifies the target device's best estimate of the LOS or NLOS of the RSRP or RSRPP of first path measurement for the resource.  This field may only be present if the field *nr-LOS-NLOS-Indicator* choice indicates *perResource*. |
| ***nr-ReportDL-PRS-MeasBasedOnSingleOrMultiHopRx***  This field indicates that the reported measurement is based on receiving single or multiple hops of DL-PRS. |

#### – *NR-DL-AoD-LocationInformation*

The IE *NR-DL-AoD-LocationInformation* is included by the target device when location information derived using NR DL-AoD is provided to the location server.

-- ASN1START

NR-DL-AoD-LocationInformation-r16 ::= SEQUENCE {

measurementReferenceTime-r16 CHOICE {

sfn-time-r16 NR-TimeStamp-r16,

utc-time-r16 UTCTime,

...

} OPTIONAL,

...,

[[

locationCoordinates-r17 LocationCoordinates OPTIONAL, -- Cond batch1

locationSource-r17 LocationSource-r13 OPTIONAL -- Cond batch2

]]

}

-- ASN1STOP

| Conditional presence | Explanation |
| --- | --- |
| *batch1* | The field is mandatory present if the field *nr-DL-AoD-LocationInformationInstances* is present in IE *NR-DL-AoD-ProvideLocationInformation*; otherwise it is not present. |
| *batch2* | The field is optionally present, need ON, if the field *nr-DL-AoD-LocationInformationInstances* is present in IE *NR-DL-AoD-ProvideLocationInformation*; otherwise it is not present. |

| *NR-DL-AoD-LocationInformation* field descriptions |
| --- |
| ***measurementReferenceTime***  This field specifies the time for which the location estimate is valid. |
| ***locationCoordinates***  This field provides a location estimate using one of the geographic shapes defined in TS 23.032 [15]. NOTE 1. |
| ***locationSource***  This field provides the source positioning technology for the location estimate. NOTE 1. |

NOTE 1: In the case of *locationCoordinates* for multiple NR positioning methods are provided, the *locationCoordinates* and *locationSource* shall be present in only one of *NR-DL-TDOA-ProvideLocationInformation* or *NR-DL-AoD-ProvideLocationInformation*.

#### 6.5.11.5 NR DL-AoD Location Information Request

#### – *NR-DL-AoD-RequestLocationInformation*

The IE *NR-DL-AoD-RequestLocationInformation* is used by the location server to request NR DL-AoD location measurements from a target device.

-- ASN1START

NR-DL-AoD-RequestLocationInformation-r16 ::= SEQUENCE {

nr-AssistanceAvailability-r16 BOOLEAN,

nr-DL-AoD-ReportConfig-r16 NR-DL-AoD-ReportConfig-r16,

...,

[[

multiMeasInSameReport-r17 ENUMERATED { requested } OPTIONAL -- Need ON

]],

[[

nr-DL-PRS-RxHoppingRequest-r18 SEQUENCE {

nr-DL-PRS-RxHoppingTotalBandwidth-r18 CHOICE {

fr1 ENUMERATED {mhz40, mhz50, mhz80, mhz100},

fr2 ENUMERATED {mhz100, mhz200, mhz400}

} OPTIONAL -- Need ON

} OPTIONAL -- Need ON

]]

}

NR-DL-AoD-ReportConfig-r16 ::= SEQUENCE {

maxDL-PRS-RSRP-MeasurementsPerTRP-r16 INTEGER (1..8) OPTIONAL, -- Need ON

...,

[[

maxDL-PRS-RSRP-MeasurementsPerTRP-r17 INTEGER (9..24) OPTIONAL, -- Need ON

maxDL-PRS-RSRPP-MeasurementsPerTRP-r17 INTEGER (1..24) OPTIONAL, -- Need ON

nr-los-nlos-IndicatorRequest-r17 SEQUENCE {

type-r17 LOS-NLOS-IndicatorType1-r17,

granularity-r17

LOS-NLOS-IndicatorGranularity1-r17,

...

} OPTIONAL, -- Need ON

reducedDL-PRS-ProcessingSamples-r17 ENUMERATED { requested, ... }

OPTIONAL, -- Need ON

lowerRxBeamSweepingFactor-FR2-r17 ENUMERATED { requested } OPTIONAL -- Need ON

]],

[[

nr-DL-PRS-MeasurementTimeWindowsConfig-r18

NR-DL-PRS-MeasurementTimeWindowsConfig-r18 OPTIONAL -- Need ON

]]

}

-- ASN1STOP

| *NR-DL-AoD-RequestLocationInformation* field descriptions |
| --- |
| ***nr-AssistanceAvailability***  This field indicates whether the target device may request additional DL-PRS assistance data from the server. TRUE means allowed and FALSE means not allowed. |
| ***multiMeasInSameReport***  This field, if present, indicates that the target device is requested to provide multiple measurement instances in a single measurement report; i.e., include the *nr-DL-AoD-SignalMeasurementInstances* (in the case of UE-assisted mode is requested) or *nr-DL-AoD-LocationInformationInstances* (in the case of UE-based mode is requested) in IE *NR-DL-AoD-ProvideLocationInformation.* |
| ***nr-DL-PRS-RxHoppingRequest***  This field, if present, indicates that the target device is requested to perform DL-PRS Rx hopping for performing RSRP or RSRPP measurements and report the hopping information used for performing the measurements. |
| ***nr-DL-PRS-RxHoppingTotalBandwidth***  This field, if present, indicates the total bandwidth of all hops in MHz. If the configured value *nr-DL-PRS-RxHoppingTotalBandwidth* is larger than the configured DL-PRS bandwidth in the provided assistance data, the UE shall assume that the actual nr-*DL-PRS-RxHoppingTotalBandwidth* is equal to the width of the configured DL-PRS in the provided assistance data. |
| ***maxDL-PRS-RSRP-MeasurementsPerTRP***  This field specifies the maximum number of DL-PRS RSRP measurements on different DL-PRS Resources from the same TRP. If this field with -r17 suffix is present, the field with -r16 suffix should not be present. |
| ***maxDL-PRS-RSRPP-MeasurementsPerTRP***  This field specifies the maximum number of DL-PRS RSRPP measurements on different DL-PRS Resources from the same TRP. |
| ***nr-los-nlos-IndicatorRequest***  This field, if present, indicates that the target device is requested to provide the indicated type and granularity of the estimated *LOS-NLOS-Indicator* in the *NR-DL-AoD-SignalMeasurementInformation*. |
| ***reducedDL-PRS-ProcessingSamples***  This field, if present and set to '*requested*', indicates that the target device is requested to perform the requested measurements with reduced number of samples (M=1 or M=2) as specified in TS 38.133 [46]. |
| ***lowerRxBeamSweepingFactor-FR2***  This field, if present, indicates that the target device is requested to use a lower Rx beam sweeping factor than 8 for FR2 according to UE's capability. |
| ***nr-DL-PRS-MeasurementTimeWindowsConfig***  This field indicates DL-PRS Resource Set(s) occurring within time window(s) for performing measurements where the time window is indicated by a start time, periodicity, offset and duration. |

#### 6.5.11.6 NR DL-AoD Capability Information

#### – *NR-DL-AoD-ProvideCapabilities*

The IE *NR-DL-AoD-ProvideCapabilities* is used by the target device to indicate its capability to support NR DL-AoD and to provide its NR DL-AoD positioning capabilities to the location server.

-- ASN1START

NR-DL-AoD-ProvideCapabilities-r16 ::= SEQUENCE {

nr-DL-AoD-Mode-r16 PositioningModes,

nr-DL-AoD-PRS-Capability-r16 NR-DL-PRS-ResourcesCapability-r16,

nr-DL-AoD-MeasurementCapability-r16 NR-DL-AoD-MeasurementCapability-r16,

nr-DL-PRS-QCL-ProcessingCapability-r16 NR-DL-PRS-QCL-ProcessingCapability-r16,

nr-DL-PRS-ProcessingCapability-r16 NR-DL-PRS-ProcessingCapability-r16,

periodicalReporting-r16 PositioningModes OPTIONAL,

...,

[[

ten-ms-unit-ResponseTime-r17 PositioningModes OPTIONAL,

nr-PosCalcAssistanceSupport-r17 BIT STRING { trpLocSup (0),

beamInfoSup (1),

rtdInfoSup (2),

beamAntInfoSup (3),

nr-IntegrityBoundsSup-r18 (4)

} (SIZE (1..8)) OPTIONAL,

nr-los-nlos-AssistanceDataSupport-r17 SEQUENCE {

type-r17 LOS-NLOS-IndicatorType2-r17,

granularity-r17 LOS-NLOS-IndicatorGranularity2-r17,

...

} OPTIONAL,

nr-DL-PRS-ExpectedAoD-or-AoA-Sup-r17 BIT STRING { eAoD (0),

eAoA (1)

} (SIZE (1..8)) OPTIONAL,

dl-PRS-ResourcePrioritySubset-Sup-r17 ENUMERATED { sameSet, differentSet, sameOrDifferentSet }

OPTIONAL,

nr-DL-PRS-BeamInfoSup-r17 ENUMERATED { supported } OPTIONAL,

nr-DL-AoD-On-Demand-DL-PRS-Support-r17 NR-On-Demand-DL-PRS-Support-r17 OPTIONAL,

nr-los-nlos-IndicatorSupport-r17 SEQUENCE {

type-r17 LOS-NLOS-IndicatorType2-r17,

granularity-r17 LOS-NLOS-IndicatorGranularity2-r17,

...

} OPTIONAL,

scheduledLocationRequestSupported-r17 ScheduledLocationTimeSupportPerMode-r17

OPTIONAL,

nr-dl-prs-AssistanceDataValidity-r17 SEQUENCE {

area-validity-r17 INTEGER (1..maxNrOfAreas-r17) OPTIONAL,

...

} OPTIONAL,

multiMeasInSameMeasReport-r17 ENUMERATED { supported } OPTIONAL,

mg-ActivationRequest-r17 ENUMERATED { supported } OPTIONAL

]],

[[

posMeasGapSupport-r17 ENUMERATED { supported } OPTIONAL

]],

[[

multiLocationEstimateInSameMeasReport-r17 ENUMERATED { supported } OPTIONAL

]],

[[

locationCoordinateTypes-r18 LocationCoordinateTypes OPTIONAL,

nr-IntegrityAssistanceSupport-r18 BIT STRING {

serviceParametersSup (0),

serviceAlertSup (1),

riskParametersSup (2),

integrityParaTRP-LocSup (3),

integrityParaBeamInfoSup (4),

integrityParaRTD-InfoSup (5),

integrityBeamAntInfoSup (6)

} (SIZE (1..8)) OPTIONAL,

periodicReportingIntervalMsSupport-r18 PeriodicReportingIntervalMsSupportPerMode-r18

OPTIONAL

]]

}

-- ASN1STOP

|  |
| --- |
| *NR-DL-AoD-ProvideCapabilities* field descriptions |
| ***nr-DL-AoD-Mode***  This field specifies the NR DL-AoD mode(s) supported by the target device. |
| ***periodicalReporting***  This field, if present, specifies the positioning modes for which the target device supports *periodicalReporting.* This is represented by a bit string, with a one‑value at the bit position means *periodicalReporting* for the positioning mode is supported; a zero‑value means not supported. If this field is absent, the target device does not support *periodicalReporting* in *CommonIEsRequestLocationInformation*. |
| ***ten-ms-unit-ResponseTime***  This field, if present, specifies the positioning modes for which the target device supports the enumerated value '*ten-milli-seconds*' in the IE *ResponseTime* in IE *CommonIEsRequestLocationInformation*. This is represented by a bit string, with a one‑value at the bit position means '*ten-milli-seconds'* response time unit for the positioning mode is supported; a zero‑value means not supported. If this field is absent, the target device does not support '*ten-milli-seconds'* response time unitin *CommonIEsRequestLocationInformation*. |
| ***nr-PosCalcAssistanceSupport***  This field indicates the Position Calculation Assistance Data supported by the target device for UE-based DL-AoD. This is represented by a bit string, with a one‑value at the bit position means the particular assistance data is supported; a zero‑value means not supported.  - bit 0 indicates whether the field *nr-TRP-LocationInfo* in IE *NR-PositionCalculationAssistance* is supported or not;  - bit 1 indicates whether the field *nr-DL-PRS-BeamInfo* in IE *NR-PositionCalculationAssistance* is supported or not;  - bit 2 indicates whether the field *nr-RTD-Info* in IE *NR-PositionCalculationAssistance* is supported or not. The UE can indicate this bit only if the UE supports *prs-ProcessingCapabilityBandList* and any of *maxNrOfDL-PRS-ResourceSetPerTrpPerFrequencyLayer*, *maxNrOfTRP-AcrossFreqs*, *maxNrOfPosLayer*, *maxNrOfDL-PRS-ResourcesPerResourceSet* and *maxNrOfDL-PRS-ResourcesPerPositioningFrequencylayer*. Otherwise, the UE does not include this field;  - bit 3 indicates whether the field *nr-TRP-BeamAntennaInfo* in IE *NR-PositionCalculationAssistance* is supported or not;  - bit 4 indicates whether the target service supports the range of integrity risk (IR) for which the integrity assistance data are valid;  - bit 5 together with bit 0 indicates whether the fields *nr-IntegrityTRP-LocationBounds, nr-IntegrityDL-PRS-ResourceSetARP-LocationBounds, nr-IntegrityDL-PRS-ResourceARP-LocationBounds* in IE *NR-TRP-LocationInfo* are supported or not; bit 5 together with bit 1 indicates whether the field *nr-IntegrityBeamInfoBounds* in IE *NR-DL-PRS-BeamInfo* is supported or not; bit 5 together with bit 2 indicates whether the field *nr-IntegrityRTD-InfoBounds* in IE *NR-RTD-Info* is supported or not; bit 5 together with bit 3 indicates whether the field *nr-integrityBeamPowerBounds* in IE *NR-TRP-BeamAntennaInfo* is supported or not. |
| ***nr-los-nlos-AssistanceDataSupport***  This field, if present, indicates that the target device supports the *NR-DL-PRS-ExpectedLOS-NLOS-Assistance* in IE *NR-PositionCalculationAssistance*:  - *type* indicates whether the target device supports '*hard*' value or '*hard*' and '*soft*' value in *LOS-NLOS-Indicator* in IE *NR-DL-PRS-ExpectedLOS-NLOS-Assistance*.  - *granularity* indicates whether the target device supports *nr-los-nlos-indicator* in IE *NR-DL-PRS-ExpectedLOS-NLOS-Assistanc*e 'per-trp', '*per-resource*', or both.  The UE can include this field only if the UE supports one of *maxDL-PRS-RSRP-MeasurementFR1*, *maxDL-PRS-RSRP-MeasurementFR2,dl-RSTD-MeasurementPerPairOfTRP-FR1, dl-RSTD-MeasurementPerPairOfTRP-FR2, maxNrOfRx-TX-MeasFR1, maxNrOfRx-TX-MeasFR2, supportOfRSRP-MeasFR1* and *supportOfRSRP-MeasFR2* . Otherwise, the UE does not include this field. |
| ***nr-DL-PRS-ExpectedAoD-or-AoA-Sup***  This field, if present, indicates that the target device supports the *NR-DL-PRS-ExpectedAoD-or-AoA* in *NR-DL-PRS-AssistanceData.* |
| ***dl-PRS-ResourcePrioritySubset-Sup***  This field, if present, indicates that the target device supports the *DL-PRS-ResourcePrioritySubset* in IE *NR-DL-PRS-Info.* Enumerated value indicates the supported resource set relationship for the target DL-PRS Resource and the associated subset. | |
| ***nr-DL-PRS-BeamInfoSup***  This field, if present, indicates that the target device supports the *NR-DL-PRS-BeamInfo* in IE *NR-DL-AoD-ProvideAssistanceData.* |
| ***nr-DL-AoD-On-Demand-DL-PRS-Support***  This field, if present, indicates that the target device supports on-demand DL-PRS requests. |
| ***nr-los-nlos-IndicatorSupport***  This field, if present, indicates that the target device supports *nr-los-nlos-Indicator* reporting in IE *NR-DL-AoD-SignalMeasurementInformation*.  - *type* indicates whether the target device supports '*hard*' value or '*hard*' and '*soft*' value in IE *LOS-NLOS-Indicator.*  - *granularit*y indicates whether the target device supports *LOS-NLOS-Indicator* reporting per TRP, per DL-PRS Resource, or both. |
| ***scheduledLocationRequestSupported***  This field, if present, specifies the positioning modes for which the target device supports scheduled location requests – i.e., supports the IE *ScheduledLocationTime* in IE *CommonIEsRequestLocationInformation* – and the time base(s) supported for the scheduled location time for each positioning mode. If this field is absent, the target device does not support scheduled location requests. |
| ***nr-dl-prs-AssistanceDataValidity***  This field, if present, indicates that the target device supports validity conditions for pre-configured assistance data and comprises the following subfields:  - ***area-validity*** indicates that the target device supports pre-configured assistance data with area validity. The integer number indicates the maximum number of areas the target device supports. |
| ***multiMeasInSameMeasReport***  This field, if present, indicates that the target device supports multiple measurement instances in a single measurement report. |
| ***mg-ActivationRequest***  This field, if present, indicates that the target device supports UL MAC CE for positioning measurement gap activation/deactivation request for DL-PRS measurements. The UE can include this field only if the UE supports *mg-ActivationRequestPRS-Meas* and *mg-ActivationCommPRS-Meas* defined in TS 38.331 [35]. |
| ***posMeasGapSupport***  This field, if present, indicates that the target device supports pre-configured positioning measurement gap for DL-PRS measurements. The UE can include this field only if the UE supports *mg-ActivationCommPRS-Meas* defined in TS 38.331 [35]. |
| ***multiLocationEstimateInSameMeasReport***  This field, if present, indicates that the target device supports multiple location estimate instances in a single measurement report. |
| ***locationCoordinateTypes***  This field indicates the geographical location coordinate types that a target device supports for UE-based DL-AoD. TRUE indicates that a location coordinate type is supported and FALSE that it is not. |
| ***nr-IntegrityAssistanceSupport***  This field indicates the Integrity Assistance Data supported. This is represented by a bit string, with a one‑value at the bit position means the particular assistance data is supported; a zero‑value means not supported.  - bit 0 indicates whether the field *nr-IntegrityServiceParameters* in IE *NR-PositionCalculationAssistance* is supported or not;  - bit 1 indicates whether the field *nr-IntegrityServiceAlert* in IE *NR-PositionCalculationAssistance* is supported or not;  - bit 2 indicates whether the field *nr-IntegrityRiskParameters* in IE *NR-PositionCalculationAssistance* is supported or not;  - bit 3 indicates whether the field *nr-IntegrityParametersTRP-LocationInfo* in IE *NR-PositionCalculationAssistance* is supported or not;  - bit 4 indicates whether the field *nr-IntegrityParametersDL-PRS-BeamInfo* in IE *NR-PositionCalculationAssistance* is supported or not;  - bit 5 indicates whether the field *nr-IntegrityParametersRTD-Info* in IE *NR-PositionCalculationAssistance* is supported or not;  - bit 6 indicates whether the field *nr-IntegrityParametersTRP-BeamAntennaInfo* in IE *NR-PositionCalculationAssistance* is supported or not. |
| ***periodicReportingIntervalMsSupport***  This field, if present, specified the supported minimum millisecond periodic reporting interval for location information per positioning mode – i.e., supports the subfield *reportingIntervalMs* of the IE *PeriodicalReportingCriteriaExt* in IE *CommonIEsRequestLocationInformation* – and the minimum millisecond report interval supported for the periodic reporting. |

#### 6.5.11.6a NR DL-AoD Capability Information Elements

#### *– NR-DL-AoD-MeasurementCapability*

The IE *NR-DL-AoD-MeasurementCapability* defines the DL-AoD measurement capability. The UE can include this IE only if the UE supports *NR-DL-PRS-ResourcesCapability* for DL-AoD. Otherwise, the UE does not include this IE;

-- ASN1START

NR-DL-AoD-MeasurementCapability-r16 ::= SEQUENCE {

maxDL-PRS-RSRP-MeasurementFR1-r16 INTEGER (1..8),

maxDL-PRS-RSRP-MeasurementFR2-r16 INTEGER (1..8),

dl-AoD-MeasCapabilityBandList-r16 SEQUENCE (SIZE (1..nrMaxBands-r16)) OF

DL-AoD-MeasCapabilityPerBand-r16,

...,

[[

maxDL-PRS-RSRP-MeasurementFR1-v1730 ENUMERATED { n16, n24 } OPTIONAL,

maxDL-PRS-RSRP-MeasurementFR2-v1730 ENUMERATED { n16, n24 } OPTIONAL

]]

}

DL-AoD-MeasCapabilityPerBand-r16 ::= SEQUENCE {

freqBandIndicatorNR-r16 FreqBandIndicatorNR-r16,

simul-NR-DL-AoD-DL-TDOA-r16 ENUMERATED { supported} OPTIONAL,

simul-NR-DL-AoD-Multi-RTT-r16 ENUMERATED { supported} OPTIONAL,

...,

[[

maxDL-PRS-FirstPathRSRP-MeasPerTRP-r17 ENUMERATED { n1, n2, n4, n8, n16, n24 } OPTIONAL,

dl-PRS-MeasRRC-Inactive-r17 ENUMERATED { supported } OPTIONAL

]],

[[

supportOfMeasurementsInTimeWindow-r18 BIT STRING {

rsrp (0),

rsrpp (1)

} (SIZE (1..8)) OPTIONAL,

supportOfPRS-MeasurementRRC-Idle-r18 ENUMERATED { supported } OPTIONAL

]]

}

-- ASN1STOP

|  |
| --- |
| *NR-DL-AoD-MeasurementCapability* field descriptions |
| ***maxDL-PRS-RSRP-MeasurementFR1***  Indicates the maximum number of DL-PRS RSRP measurements on different DL-PRS Resources from the same TRP supported by the UE on FR1. If this field with suffix -v1730 is present, the target device should set the field with suffix -r16 to value '8'. |
| ***maxDL-PRS-RSRP-MeasurementFR2***  Indicates the maximum number of DL-PRS RSRP measurements on different DL-PRS Resources from the same TRP supported by the UE on FR2. If this field with suffix -v1730 is present, the target device should set the field with suffix -r16 to value '8'. |
| ***simul-NR-DL-AoD-DL-TDOA***  Indicates whether the UE supports simultaneous processing for DL-AoD and DL-TDOA measurements. The UE can include this field only if the UE supports DL-TDOA and DL-AoD. Otherwise, the UE does not include this field. |
| ***simul-NR-DL-AoD-Multi-RTT***  Indicates whether the UE supports simultaneous processing for DL-AoD and UE Multi-RTT measurements. The UE can include this field only if the UE supports Multi-RTT and DL-AoD. Otherwise, the UE does not include this field. |
| ***maxDL-PRS-FirstPathRSRP-MeasPerTRP***  This field, if present, indicates that the target device supports measuring and reporting the DL-PRS RSRPP of the first path. The enumerated value indicates the maximum number of RSRPP of first path per TRP supported. The UE can include this field only if the UE supports one of *maxDL-PRS-RSRP-MeasurementFR1* and *maxDL-PRS-RSRP-MeasurementFR2*. Otherwise, the UE does not include this field.  NOTE 1: The maximum number of first path DL-PRS RSRP per TRP should be less than or equal to the maximum number of DL-PRS RSRP defined in *maxDL-PRS-RSRP-MeasurementFR1* and *maxDL-PRS-RSRP-MeasurementFR2*. |
| ***dl-PRS-MeasRRC-Inactive***  This field, if present, indicates that the target device supports DL-PRS measurement in RRC\_INACTIVE state. The UE can include this field only if the UE supports *maxNrOfDL-PRS-ResourceSetPerTrpPerFrequencyLayer, maxNrOfTRP-AcrossFreqs, maxNrOfPosLayer* and *dl-PRS-BufferType-RRC-Inactive*. Otherwise, the UE does not include this field.  NOTE 1: This capability is applicable to both, UE-assisted and UE-based DL-AoD.  NOTE 2: The capabilities *NR-DL-PRS-ResourcesCapability, simul-NR-DL-AoD-DL-TDOA* are the same in RRC\_INACTIVE state. |
| ***supportOfMeasurementsInTimeWindow***  This field, if present, indicates that the target device supports performing measurements inside the indicated time window only for DL-AoD. This is represented by a bit string, with a one‑value at the bit position means the particular measurement is supported; a zero‑value means not supported.  - bit 0 indicates whether performing DL PRS-RSRP is supported or not;  - bit 1 indicates whether performing DL PRS-RSRPP is supported or not;  The UE can include this field only if the UE supports *maxNrOfDL-PRS-ResourcesPerResourceSet* and *maxNrOfDL-PRS-ResourcesPerPositioningFrequencylayer*. Otherwise, the UE does not include this field. |
| ***supportOfPRS-MeasurementRRC-Idle***  Indicates whether the UE supports DL-PRS measurement in RRC\_IDLE for DL-AoD. The UE can include this field only if the UE supports *supportedBandwidthPRS, dl-PRS-BufferType, durationOfPRS-Processing, maxNumOfDL-PRS-ResProcessedPerSlot,* *dl-PRS-BufferType-RRC-Inactive, durationOfPRS-Processing-RRC-Inactive, maxNumOfDL-PRS-ResProcessedPerSlot-RRC-Inactive* and *dl-PRS-MeasRRC-Inactive*. Otherwise, the UE does not include this field. |

#### 6.5.11.7 NR DL-AoD Capability Information Request

#### – *NR-DL-AoD-RequestCapabilities*

The IE *NR-DL-AoD-RequestCapabilities* is used by the location server to request the capability of the target device to support NR DL-AoD and to request NR DL-AoD positioning capabilities from a target device.

-- ASN1START

NR-DL-AoD-RequestCapabilities-r16 ::= SEQUENCE {

...

}

-- ASN1STOP

#### 6.5.11.8 NR DL-AoD Error Elements

#### – *NR-DL-AoD-Error*

The IE *NR-DL-AoD-Error* is used by the location server or target device to provide NR DL-AoD error reasons to the target device or location server, respectively.

-- ASN1START

NR-DL-AoD-Error-r16 ::= CHOICE {

locationServerErrorCauses-r16 NR-DL-AoD-LocationServerErrorCauses-r16,

targetDeviceErrorCauses-r16 NR-DL-AoD-TargetDeviceErrorCauses-r16,

...

}

-- ASN1STOP

#### – *NR-DL-AoD-LocationServerErrorCauses*

The IE *NR-DL-AoD-LocationServerErrorCauses* is used by the location server to provide NR DL-AoD error reasons to the target device.

-- ASN1START

NR-DL-AoD-LocationServerErrorCauses-r16 ::= SEQUENCE {

cause-r16 ENUMERATED { undefined,

assistanceDataNotSupportedByServer,

assistanceDataSupportedButCurrentlyNotAvailableByServer,

notProvidedAssistanceDataNotSupportedByServer,

...,

on-demand-dl-prs-NotSupportedByServer-v1700,

on-demand-dl-prs-SupportedButCurrentlyNotAvailableByServer-v1700

},

...

}

-- ASN1STOP

#### – *NR-DL-AoD-TargetDeviceErrorCauses*

The IE *NR-DL-AoD-TargetDeviceErrorCauses* is used by the target device to provide NR DL-AoD error reasons to the location server.

-- ASN1START

NR-DL-AoD-TargetDeviceErrorCauses-r16 ::= SEQUENCE {

cause-r16 ENUMERATED { undefined,

assistance-data-missing,

unableToMeasureAnyTRP,

attemptedButUnableToMeasureSomeNeighbourTRPs,

thereWereNotEnoughSignalsReceivedForUeBasedDL-AoD,

locationCalculationAssistanceDataMissing,

...

},

...,

[[

remoteUE-Indication-r18 ENUMERATED {true} OPTIONAL -- Cond NR

]]

}

-- ASN1STOP

| Conditional presence | Explanation |
| --- | --- |
| *NR* | This field is optionally present, need OR, for NR access. Otherwise it is not present. |

| *NR-DL-AoD-TargetDeviceErrorCauses* field descriptions |
| --- |
| ***remoteUE-Indication***  This field indicates whether the target device in NR access is configured as a L2 U2N Remote UE. |

### 6.5.12 NR Multi-RTT Positioning

This clause defines the information elements for NR Multi-RTT positioning (TS 38.305 [40]).

#### 6.5.12.1 NR Multi-RTT Assistance Data

#### – *NR-Multi-RTT-ProvideAssistanceData*

The IE *NR-Multi-RTT-ProvideAssistanceData* is used by the location server to provide assistance data to enable UE‑assisted NR Multi-RTT. It may also be used to provide NR Multi-RTT positioning specific error reason.

-- ASN1START

NR-Multi-RTT-ProvideAssistanceData-r16 ::= SEQUENCE {

nr-DL-PRS-AssistanceData-r16 NR-DL-PRS-AssistanceData-r16 OPTIONAL, -- Need ON

nr-SelectedDL-PRS-IndexList-r16 NR-SelectedDL-PRS-IndexList-r16 OPTIONAL, -- Need ON

nr-Multi-RTT-Error-r16 NR-Multi-RTT-Error-r16 OPTIONAL, -- Need ON

...,

[[

nr-On-Demand-DL-PRS-Configurations-r17 NR-On-Demand-DL-PRS-Configurations-r17

OPTIONAL, -- Need ON

nr-On-Demand-DL-PRS-Configurations-Selected-IndexList-r17

NR-On-Demand-DL-PRS-Configurations-Selected-IndexList-r17

OPTIONAL, -- Need ON

assistanceDataValidityArea-r17 AreaID-CellList-r17 OPTIONAL -- Need ON

]]

}

-- ASN1STOP

|  |
| --- |
| *NR-Multi-RTT-ProvideAssistanceData* field descriptions |
| ***nr-DL-PRS-AssistanceData***  This field specifies the assistance data reference and neighbour TRPs and provides the DL-PRS configuration for the TRPs.  Note, if this field is absent but the *nr-SelectedDL-PRS-IndexList* field is present, the *nr-DL-PRS-AssistanceData* may be provided in IE *NR-DL-TDOA-ProvideAssistanceData* or *NR-DL-AoD-ProvideAssistanceData*. |
| ***nr-SelectedDL-PRS-IndexList***  This field specifies the DL-PRS Resources which are applicable for this *NR-Multi-RTT-ProvideAssistanceData* message. |
| ***nr-Multi-RTT-Error***  This field provides Multi-RTT error reasons. |
| ***nr-On-Demand-DL-PRS-Configurations***  This field provides a set of available DL-PRS configurations which can be requested by the target device on-demand.  NOTE 1: Void.  NOTE 2: If this field is absent but the *nr-On-Demand-DL-PRS-Configurations-Selected-IndexList* is present, the *nr-On-Demand-DL-PRS-Configurations* may be provided in *IE NR-DL-AoD-ProvideAssistanceData* or *NR-DL-TDOA-ProvideAssistanceData*. |
| ***nr-On-Demand-DL-PRS-Configurations-Selected-IndexList***  This field specifies the selected available on-demand DL-PRS configurations which are applicable for this *NR-Multi-RTT-ProvideAssistanceData message*. |
| ***assistanceDataValidityArea***  This field specifies the network area for which this *NR-Multi-RTT-ProvideAssistanceData* is valid. |

#### 6.5.12.2 NR Multi-RTT Assistance Data Request

#### – *NR-Multi-RTT-RequestAssistanceData*

The IE *NR-Multi-RTT-RequestAssistanceData* is used by the target device to request assistance data from a location server.

-- ASN1START

NR-Multi-RTT-RequestAssistanceData-r16 ::= SEQUENCE {

nr-PhysCellID-r16 NR-PhysCellID-r16 OPTIONAL,

nr-AdType-r16 BIT STRING { dl-prs (0),

ul-srs (1) } (SIZE (1..8)),

...,

[[

nr-on-demand-DL-PRS-Request-r17 NR-On-Demand-DL-PRS-Request-r17 OPTIONAL,

nr-DL-PRS-ExpectedAoD-or-AoA-Request-r17 ENUMERATED { eAoD, eAoA } OPTIONAL,

pre-configured-AssistanceDataRequest-r17 ENUMERATED { true } OPTIONAL

]]

}

-- ASN1STOP

| *NR-Multi-RTT-RequestAssistanceData* field descriptions |
| --- |
| ***nr-PhysCellID***  This field specifies the NR physical cell identity of the current primary cell of the target device. |
| ***nr-AdType***  This field indicates the requested assistance data and/or configuration. *dl-prs* means requested assistance data is *nr-DL-PRS-AssistanceData*, *ul-srs* means a request for UL-SRS configuration.  NOTE: UL-SRS is configured via NRPPa and RRC signalling as specified in clause 8.10.4 of TS 38.305 [40]. |
| ***nr-on-demand-DL-PRS-Request***  This field indicates the on-demand DL-PRS requested for Multi-RTT. This field may be included when the *dl-prs* bit in *nr-AdType* is set to value '1'. |
| ***nr-DL-PRS-ExpectedAoD-or-AoA-Request***  This field, if present, indicates that the IE *NR-DL-PRS-ExpectedAoD-or-AoA* in *NR-DL-PRS-AssistanceData* is requested. Enumerated value '*eAoD*' indicates that expected AoD information is requested; value 'eAoA' indicates that expected AoA information is requested.  This field may only be present if the '*dl-prs*' bit in *nr-AdType* is set to value '1'. |
| ***pre-configured-AssistanceDataRequest***  This field, if present, indicates that the target device requests pre-configured assistance data with area validity. |

#### 6.5.12.3 NR Multi-RTT Location Information

#### – *NR-Multi-RTT-ProvideLocationInformation*

The IE *NR-Multi-RTT-ProvideLocationInformation* is used by the target device to provide NR Multi-RTT location measurements to the location server. It may also be used to provide NR Multi-RTT positioning specific error reason.

-- ASN1START

NR-Multi-RTT-ProvideLocationInformation-r16 ::= SEQUENCE {

nr-Multi-RTT-SignalMeasurementInformation-r16

NR-Multi-RTT-SignalMeasurementInformation-r16

OPTIONAL,

nr-Multi-RTT-Error-r16 NR-Multi-RTT-Error-r16 OPTIONAL,

...,

[[

nr-Multi-RTT-SignalMeasurementInstances-r17

SEQUENCE (SIZE (1..maxMeasInstances-r17)) OF

NR-Multi-RTT-SignalMeasurementInformation-r16

OPTIONAL --Cond batchUEA

]]

}

-- ASN1STOP

| Conditional presence | Explanation |
| --- | --- |
| *batchUEA* | The field is optionally present if the field *nr-Multi-RTT-SignalMeasurementInformation* is absent; otherwise it is not present. |

#### 6.5.12.4 NR Multi-RTT Location Information Elements

#### – *NR-Multi-RTT-SignalMeasurementInformation*

The IE *NR-Multi-RTT-SignalMeasurementInformation* is used by the target device to provide NR Multi-RTT measurements to the location server.

-- ASN1START

NR-Multi-RTT-SignalMeasurementInformation-r16 ::= SEQUENCE {

nr-Multi-RTT-MeasList-r16 NR-Multi-RTT-MeasList-r16,

nr-NTA-Offset-r16 ENUMERATED { nTA1, nTA2, nTA3, nTA4, ... } OPTIONAL,

...,

[[

nr-SRS-TxTEG-Set-r17 SEQUENCE (SIZE(1..maxTxTEG-Sets-r17)) OF

NR-SRS-TxTEG-Element-r17 OPTIONAL

-- Cond Case2-3

]],

[[

nr-UE-RxTEG-TimingErrorMargin-r17 TEG-TimingErrorMargin-r17 OPTIONAL,-- Cond TEGCase3

nr-UE-TxTEG-TimingErrorMargin-r17 TEG-TimingErrorMargin-r17 OPTIONAL,-- Cond TEGCase2-3

nr-UE-RxTxTEG-TimingErrorMargin-r17 RxTxTEG-TimingErrorMargin-r17 OPTIONAL -- Cond TEGCase1-2

]]

}

NR-Multi-RTT-MeasList-r16 ::= SEQUENCE (SIZE(1..nrMaxTRPs-r16)) OF NR-Multi-RTT-MeasElement-r16

NR-Multi-RTT-MeasElement-r16 ::= SEQUENCE {

dl-PRS-ID-r16 INTEGER (0..255),

nr-PhysCellID-r16 NR-PhysCellID-r16 OPTIONAL,

nr-CellGlobalID-r16 NCGI-r15 OPTIONAL,

nr-ARFCN-r16 ARFCN-ValueNR-r15 OPTIONAL,

nr-DL-PRS-ResourceID-r16 NR-DL-PRS-ResourceID-r16 OPTIONAL,

nr-DL-PRS-ResourceSetID-r16 NR-DL-PRS-ResourceSetID-r16 OPTIONAL,

nr-UE-RxTxTimeDiff-r16 CHOICE {

k0-r16 INTEGER (0..1970049),

k1-r16 INTEGER (0..985025),

k2-r16 INTEGER (0..492513),

k3-r16 INTEGER (0..246257),

k4-r16 INTEGER (0..123129),

k5-r16 INTEGER (0..61565),

...,

kMinus6-r18 INTEGER (0..126083073),

kMinus5-r18 INTEGER (0..63041537),

kMinus4-r18 INTEGER (0..31520769),

kMinus3-r18 INTEGER (0..15760385),

kMinus2-r18 INTEGER (0..7880193),

kMinus1-r18 INTEGER (0..3940097)

},

nr-AdditionalPathList-r16 NR-AdditionalPathList-r16 OPTIONAL,

nr-TimeStamp-r16 NR-TimeStamp-r16,

nr-TimingQuality-r16 NR-TimingQuality-r16,

nr-DL-PRS-RSRP-Result-r16 INTEGER (0..126) OPTIONAL,

nr-Multi-RTT-AdditionalMeasurements-r16

NR-Multi-RTT-AdditionalMeasurements-r16 OPTIONAL,

...,

[[

nr-UE-RxTx-TEG-Info-r17 NR-UE-RxTx-TEG-Info-r17 OPTIONAL,

nr-DL-PRS-FirstPathRSRP-Result-r17 INTEGER (0..126) OPTIONAL,

nr-los-nlos-Indicator-r17 CHOICE {

perTRP-r17 LOS-NLOS-Indicator-r17,

perResource-r17 LOS-NLOS-Indicator-r17

} OPTIONAL,

nr-AdditionalPathListExt-r17 NR-AdditionalPathListExt-r17 OPTIONAL,

nr-Multi-RTT-AdditionalMeasurementsExt-r17

NR-Multi-RTT-AdditionalMeasurementsExt-r17 OPTIONAL

]],

[[

nr-MeasBasedOnAggregatedResources-r18 ENUMERATED {true} OPTIONAL,

nr-AggregatedDL-PRS-ResourceInfo-List-r18 SEQUENCE (SIZE (2..3)) OF

NR-AggregatedDL-PRS-ResourceInfo-Element-r18 OPTIONAL,

nr-RSCP-r18 INTEGER (0..3599) OPTIONAL,

nr-PhaseQuality-r18 NR-PhaseQuality-r18 OPTIONAL,

nr-RSCP-AddSampleMeasurements-r18

SEQUENCE (SIZE (1..nrNumOfSamples-1-r18 )) OF NR-RSCP-AdditionalMeasurements-r18

OPTIONAL,

nr-ReportDL-PRS-MeasBasedOnSingleOrMultiHopRx-r18

ENUMERATED { singleHop, multipleHop } OPTIONAL,

nr-NTN-UE-RxTxMeasurements-r18 NR-NTN-UE-RxTxMeasurements-r18 OPTIONAL

]]

}

NR-Multi-RTT-AdditionalMeasurements-r16 ::= SEQUENCE (SIZE (1..3)) OF

NR-Multi-RTT-AdditionalMeasurementElement-r16

NR-Multi-RTT-AdditionalMeasurementsExt-r17 ::= SEQUENCE (SIZE (1..maxAddMeasRTT-r17)) OF

NR-Multi-RTT-AdditionalMeasurementElement-r16

NR-Multi-RTT-AdditionalMeasurementElement-r16 ::= SEQUENCE {

nr-DL-PRS-ResourceID-r16 NR-DL-PRS-ResourceID-r16 OPTIONAL,

nr-DL-PRS-ResourceSetID-r16 NR-DL-PRS-ResourceSetID-r16 OPTIONAL,

nr-DL-PRS-RSRP-ResultDiff-r16 INTEGER (0..61) OPTIONAL,

nr-UE-RxTxTimeDiffAdditional-r16 CHOICE {

k0-r16 INTEGER (0..8191),

k1-r16 INTEGER (0..4095),

k2-r16 INTEGER (0..2047),

k3-r16 INTEGER (0..1023),

k4-r16 INTEGER (0..511),

k5-r16 INTEGER (0..255),

...,

kMinus6-r18 INTEGER (0..524224),

kMinus5-r18 INTEGER (0..262112),

kMinus4-r18 INTEGER (0..131056),

kMinus3-r18 INTEGER (0..65528),

kMinus2-r18 INTEGER (0..32764),

kMinus1-r18 INTEGER (0..16382)

},

nr-TimingQuality-r16 NR-TimingQuality-r16,

nr-AdditionalPathList-r16 NR-AdditionalPathList-r16 OPTIONAL,

nr-TimeStamp-r16 NR-TimeStamp-r16,

...,

[[

nr-UE-RxTx-TEG-Info-r17 NR-UE-RxTx-TEG-Info-r17 OPTIONAL,

nr-DL-PRS-FirstPathRSRP-ResultDiff-r17 INTEGER (0..61) OPTIONAL,

nr-los-nlos-IndicatorPerResource-r17 LOS-NLOS-Indicator-r17 OPTIONAL,

nr-AdditionalPathListExt-r17 NR-AdditionalPathListExt-r17 OPTIONAL

]],

[[

nr-MeasBasedOnAggregatedResources-r18 ENUMERATED {true} OPTIONAL,

nr-AggregatedDL-PRS-ResourceInfo-List-r18 SEQUENCE (SIZE (2..3)) OF

NR-AggregatedDL-PRS-ResourceInfo-Element-r18 OPTIONAL,

nr-RSCP-r18 INTEGER (0..3599) OPTIONAL,

nr-PhaseQuality-r18 NR-PhaseQuality-r18 OPTIONAL,

nr-RSCP-AdditionalMeasurementsAddSample-r18

SEQUENCE (SIZE (1..nrNumOfSamples-1-r18 )) OF NR-RSCP-AdditionalMeasurements-r18

OPTIONAL,

nr-ReportDL-PRS-MeasBasedOnSingleOrMultiHopRx-r18

ENUMERATED { singleHop, multipleHop } OPTIONAL,

nr-NTN-UE-RxTxMeasurements-r18 NR-NTN-UE-RxTxMeasurements-r18 OPTIONAL

]]

}

NR-SRS-TxTEG-Element-r17 ::= SEQUENCE {

nr-TimeStamp-r17 NR-TimeStamp-r16 OPTIONAL, -- Need OP

nr-UE-Tx-TEG-ID-r17 INTEGER (0..maxNumOfTxTEGs-1-r17),

carrierFreq-r17 SEQUENCE {

absoluteFrequencyPointA-r17 ARFCN-ValueNR-r15,

offsetToPointA-r17 INTEGER (0..2199)

} OPTIONAL,

srs-PosResourceList-r17 SEQUENCE (SIZE (1..maxNumOfSRS-PosResources-r17)) OF

INTEGER (0..maxNumOfSRS-PosResources-1-r17),

...

}

NR-UE-RxTx-TEG-Info-r17 ::= CHOICE {

case1-r17 SEQUENCE {

nr-UE-RxTx-TEG-ID-r17 INTEGER (0..maxNumOfRxTxTEGs-1-r17)

},

case2-r17 SEQUENCE {

nr-UE-RxTx-TEG-ID-r17 INTEGER (0..maxNumOfRxTxTEGs-1-r17),

nr-UE-Tx-TEG-Index-r17 INTEGER (1..maxTxTEG-Sets-r17)

},

case3-r17 SEQUENCE {

nr-UE-Rx-TEG-ID-r17 INTEGER (0..maxNumOfRxTEGs-1-r17),

nr-UE-Tx-TEG-Index-r17 INTEGER (1..maxTxTEG-Sets-r17)

},

...

}

NR-RSCP-AdditionalMeasurements-r18 ::= SEQUENCE {

nr-RSCP-r18 INTEGER (0..3599) OPTIONAL,

nr-PhaseQuality-r18 NR-PhaseQuality-r18 OPTIONAL,

nr-TimeStamp-r18 NR-TimeStamp-r16 OPTIONAL,

...

}

NR-NTN-UE-RxTxMeasurements-r18 ::= SEQUENCE {

nr-NTN-UE-RxTxTimeDiffSubframeOffset-r18 INTEGER (0..542),

nr-NTN-DL-TimingDrift-r18 INTEGER (-265..265)

}

-- ASN1STOP

| Conditional presence | Explanation |
| --- | --- |
| *Case2-3* | The field is mandatory present if the IE *NR-UE-RxTx-TEG-Info* is provided for choice's *case2* and *case3*. Otherwise it is not present. |
| *TEGCase3* | The field is optionally present, need OP, if the IE *NR-UE-RxTx-TEG-Info* is provided for choice *case3*. Otherwise it is not present. |
| *TEGCase2-3* | The field is optionally present, need OP, if the IE *NR-UE-RxTx-TEG-Info* is provided for choice's *case2* and *case3*. Otherwise it is not present. |
| *TEGCase1-2* | The field is optionally present, need OP, if the IE *NR-UE-RxTx-TEG-Info* is provided for choice's *case1* and *case2*. Otherwise it is not present. |

|  |
| --- |
| *NR-Multi-RTT-SignalMeasurementInformation* field descriptions |
| ***nr-NTA-Offset***  This field provides the *NTAoffset* used by the target device as specified in TS 38.133 [46], Table 7.1.2-2. Enumerated values nTA1, nTA2, nTA3, and nTA4 correspond to *NTAoffset* of 25600 Tc, 0 Tc, 39936 Tc, and 13792 Tc, respectively. |
| ***nr-SRS-TxTEG-Set***  This field provides the SRS for Positioning Resources associated with a particular UE Tx TEG and comprises the following subfields:  - ***nr-TimeStamp*** specifies the start time for which the *NR-SRS-TxTEG-Element* is valid. If this field is absent, the *nr-TimeStamp* of this instance of the *NR-SRS-TxTEG-Element* of the *nr-SRS-TxTEG-Set* is the same as the *nr-TimeStamp* of the previous instance of the *NR-SRS-TxTEG-Element*. If this field is also absent in the first *NR-SRS-TxTEG-Element* of the *nr-SRS-TxTEG-Set*, all *NR-SRS-TxTEG-Element*'s provided are valid for the measurement period of the *NR-Multi-RTT-SignalMeasurementInformation.*  - ***nr-UE-Tx-TEG-ID*** specifies the ID of this UE Tx TEG.  - ***carrierFreq*** specifies the frequency of the SRS for positioning resources.  - ***srs-PosResourceList*** specifies the SRS for Positioning Resources belonging to this UE Tx TEG.  For each UE Tx TEG, there may be up to 8 changes (different *nr-TimeStamp*) of the TEG-SRS association information provided in *nr-SRS-TxTEG-Set*, i.e., the maximum value for *maxTxTEG-Sets* is 64. |
| ***nr-UE-RxTEG-TimingErrorMargin***  This field specifies the UE Rx TEG timing error margin value for all the UE Rx TEGs within one *NR-Multi-RTT-SignalMeasurementInformation*. If the IE *NR-UE-RxTx-TEG-Info* is present with choice *case3* and this field is absent, the receiver should consider the UE Rx TEG timing error margin value to be the maximum value available in IE *TEG-TimingErrorMargin*. |
| ***nr-UE-TxTEG-TimingErrorMargin***  This field specifies the UE Tx TEG timing error margin value for all the UE Tx TEGs within one *NR-Multi-RTT-SignalMeasurementInformation*. If the IE *NR-UE-RxTx-TEG-Info* is present with choice *case2* or *case3* and this field is absent, the receiver should consider the UE Tx TEG timing error margin value to be the maximum value available in IE *TEG-TimingErrorMargin*. |
| ***nr-UE-RxTxTEG-TimingErrorMargin***  This field specifies the UE RxTx TEG timing error margin value for all the UE RxTx TEGs within one *NR-Multi-RTT-SignalMeasurementInformation*. If the IE *NR-UE-RxTx-TEG-Info* is present with choice *case1* or *case2* and this field is absent, the receiver should consider the UE RxTx TEG timing error margin value to be the maximum applicable value as defined in TS 38.133 [46]. |
| ***dl-PRS-ID***  This field is used along with a DL-PRS Resource Set ID and a DL-PRS Resources ID to uniquely identify a DL-PRS Resource. This ID can be associated with multiple DL-PRS Resource Sets associated with a single TRP.  Each TRP should only be associated with one such ID. |
| ***nr-PhysCellID***  This field specifies the physical cell identity of the associated TRP, as defined in TS 38.331 [35]. |
| ***nr-CellGlobalID***  This field specifies the NCGI, the globally unique identity of a cell in NR, of the associated TRP, as defined in TS 38.331 [35]. |
| ***nr-ARFCN***  This field specifies the NR-ARFCN of the TRP's CD-SSB (as defined in TS 38.300 [47]) corresponding to *nr-PhysCellID*. |
| ***nr-UE-RxTxTimeDiff***  This field specifies the UE Rx–Tx time difference measurement, as defined in TS 38.215 [36]. |
| ***nr-AdditionalPathList***  This field specifies one or more additional detected path timing values for the TRP or resource, relative to the path timing used for determining the *nr-UE-RxTxTimeDiff* value. If this field was requested but is not included, it means the UE did not detect any additional path timing values. If this field is present, the field *nr-AdditionalPathListExt* shall be absent. |
| ***nr-TimeStamp***  This field specifies the time instance for which the measurement is performed. If RSCP measurement is present, the timestamp applies to both RSCP and UE Rx–Tx time difference measurement. |
| ***nr-TimingQuality***  This field specifies the target device′s best estimate of the quality of the measurement. |
| ***nr-DL-PRS-RSRP-Result***  This field specifies the NR DL-PRS reference signal received power (DL PRS-RSRP) measurement, as defined in TS 38.215 [36]. The mapping of the quantity is defined as in TS 38.133 [46]. |
| ***nr-Multi-RTT-AdditionalMeasurements***  This field provides up to 3 additional UE Rx-Tx time difference measurements corresponding to a single configured SRS Resource or Resource Set for positioning. Each measurement corresponds to a single received DL-PRS Resource or DL-PRS Resource Set [45].  If this field is present, the field *nr-Multi-RTT-AdditionalMeasurementsExt* shall be absent. |
| ***nr-UE-RxTx-TEG-Info***  This field provides the ID(s) of the UE TEG associated with the *nr-UE-RxTxTimeDiff* or*nr-UE-RxTxTimeDiffAdditional* measurement. One of the following combinations of TEG IDs can be provided:  - ***case1*** provides the UE RxTx TEG ID;  - ***case2*** provides the UE RxTx TEG ID together with the UE Tx TEG ID. The *nr-UE-Tx-TEG-Index* provides the index to the *nr-SRS-TxTEG-Set* field for the applicable UE Tx TEG ID, where value '1' indicates the first *NR-SRS-TxTEG-Element* in *nr-SRS-TxTEG-Set*, value '2' indicates the second *NR-SRS-TxTEG-Element* in *nr-SRS-TxTEG-Set*, and so on;  - ***case3*** provides the UE Rx TEG ID together with the UE Tx TEG ID. The *nr-UE-Tx-TEG-Index* provides the index to the *nr-SRS-TxTEG-Set* field for the applicable UE Tx TEG ID, where value '1' indicates the first *NR-SRS-TxTEG-Element* in *nr-SRS-TxTEG-Set*, value '2' indicates the second *NR-SRS-TxTEG-Element* in *nr-SRS-TxTEG-Set*, and so on. |
| ***nr-DL-PRS-FirstPathRSRP-Result***  This field specifies the NR DL-PRS reference signal received path power (DL PRS-RSRPP) of the first detected path in time, as defined in TS 38.215 [36]. The mapping of the measured quantity is defined as in TS 38.133 [46]. |
| ***nr-los-nlos-Indicator***  This field specifies the target device's best estimate of the LOS or NLOS of the UE Rx-Tx Time Difference, RSRP or RSRPP of first path measurement for the TRP or resource.  NOTE: If the requested type or granularity in *nr-los-nlos-IndicatorRequest* is not possible, the target device may provide a different type and granularity for the estimated *LOS-NLOS-Indicator.* |
| ***nr-AdditionalPathListExt***  This field provides up to 8 additional detected path timing values for the TRP or resource, relative to the path timing used for determining the *nr-UE-RxTxTimeDiff* value. If this field was requested but is not included, it means the UE did not detect any additional path timing values. If this field is present, the field *nr-AdditionalPathList* shall be absent. |
| ***nr-Multi-RTT-AdditionalMeasurementsExt***  This field, in addition to the measurements provided in *NR-Multi-RTT-MeasElement*, provides UE Rx-Tx time difference measurements of up to 4 DL-PRS Resources of a TRP with different UE RxTx or UE Rx TEGs. For a certain DL-PRS Resource, there can be up to 8 measurement results with respect to different UE RxTx or UE Rx TEGs. If this field is present, the field *nr-Multi-RTT-AdditionalMeasurements* shall be absent. |
| ***nr-MeasBasedOnAggregatedResources***  This field indicates whether the UE RxTx Time Difference measurement, RSRP measurement (if included), and RSRPP measurement (if included) is based on aggregated DL-PRS Resources. |
| ***nr-AggregatedDL-PRS-ResourceInfo-List***  This field provides the DL-PRS Resource Set IDs which are used for the aggregated UE Rx-Tx time difference, RSRP, or RSRPP measurement results. This field is optionally present if the field *nr-MeasBasedOnAggregatedResources* is present; otherwise, it is not present. If the field is present, the field *nr-DL-PRS-ResourceID* and *nr-DL-PRS-ResourceSetID* should not be included, and the *dl-PRS-ID* in IE *NR-Multi-RTT-MeasElement* shall be ignored by a receiver. The a*ggregatedDL-PRS-ID* in the *nr-AggregatedDL-PRS-ResourceInfo-List* is always provided for the first measurement when *nr-AggregatedDL-PRS-ResourceInfo-List* is included in *NR-Multi-RTT-MeasElement*. The a*ggregatedDL-PRS-ID* is not present in the *nr-AggregatedDL-PRS-ResourceInfo-List* when *nr-AggregatedDL-PRS-ResourceInfo-List* is included in *NR-Multi-RTT-AdditionalMeasurementElement*. |
| ***nr-RSCP***  This field specifies the NR DL reference signal carrier phase measurement, as defined in TS 38.215 [36]. Mapping of the measured quantity is defined as in TS 38.133 [46]. |
| ***nr-PhaseQuality***  This field specifies the target device′s best estimate of the quality of the RSCP measurement. |
| ***nr-RSCP-AddSampleMeasurements***  This field, in addition to the measurements provided in *NR-Multi-RTT-MeasElement*, provides up to 3 RSCP measurements associated with the *nr-UE-RxTxTimeDiff* in *NR-Multi-RTT-MeasElement*. |
| ***nr-ReportDL-PRS-MeasBasedOnSingleOrMultiHopRx***  This field indicates that the reported measurement is based on DL-PRS receive hopping with either single hop or multiple hops. |
| ***nr-DL-PRS-RSRP-ResultDiff***  This field provides the additional DL-PRS RSRP measurement result relative to *nr-DL-PRS-RSRP-Result.* The DL-PRS RSRP value of this measurement is obtained by adding the value of this field to the value of the *nr-DL-PRS-RSRP-Result*. The mapping of this field is defined as in TS 38.133 [46]. |
| ***nr-UE-RxTxTimeDiffAdditional***  This field provides the additional UE Rx-Tx Difference measurement result relative to *nr-UE-RxTxTimeDiff.* The UE Rx-Tx Difference value of this measurement is obtained by adding the value of this field to the value of the *nr-UE-RxTxTimeDiff* field. The mapping of the field is defined in TS 38.133 [46]. |
| ***nr-DL-PRS-FirstPathRSRP-ResultDiff***  This field specifies the additional NR DL-PRS reference signal received path power (DL PRS-RSRPP) of the first detected path in time relative to *nr-DL-PRS-FirstPathRSRP-Result*. The DL-PRS RSRPP of first path value of this measurement is obtained by adding the value of this field to the value of the *nr-DL-PRS-FirstPathRSRP-Result* field. The mapping of the field is defined in TS 38.133 [46]. |
| ***nr-los-nlos-IndicatorPerResource***  This field specifies the target device's best estimate of the LOS or NLOS of the UE Rx-Tx Time Difference, RSRP or RSRPP of first path measurement for the resource.  This field may only be present if the field *nr-LOS-NLOS-Indicator* choice indicates *perResource*. |
| ***nr-RSCP-AdditionalMeasurementsAddSample***  This field, provides up to 3 RSCP measurement samples associated with the UE Rx-Tx Time Difference measurement in *NR-Multi-RTT-AdditionalMeasurementElement.* |
| ***nr-NTN-UE-RxTxMeasurements***  This field provides additional measurements for the UE Rx-Tx time difference in NTN and comprises the following subfields:  - ***nr-NTN-UE-RxTxTimeDiffSubframeOffset*** specifies the UE Rx-Tx time difference subframe offset measurement in unit of subframe, as defined in TS 38.215 [36].  - ***nr-NTN-DL-TimingDrift*** specifies the DL timing drift measurement, as defined in TS 38.215 [36]. The granularity of *nr-NTN-DL-TimingDrift* is 0.1 ppm. Values are given in unit of corresponding granularity. |

#### 6.5.12.5 NR Multi-RTT Location Information Request

#### – *NR-Multi-RTT-RequestLocationInformation*

The IE *NR-Multi-RTT-RequestLocationInformation* is used by the location server to request NR Multi-RTT location measurements from a target device.

-- ASN1START

NR-Multi-RTT-RequestLocationInformation-r16 ::= SEQUENCE {

nr-UE-RxTxTimeDiffMeasurementInfoRequest-r16

ENUMERATED { true } OPTIONAL, -- Need ON

nr-RequestedMeasurements-r16 BIT STRING { prsrsrpReq (0),

firstPathRsrpReq-r17 (1),

dl-PRS-RSCP-Request-r18 (2)}

(SIZE(1..8)),

nr-AssistanceAvailability-r16 BOOLEAN,

nr-Multi-RTT-ReportConfig-r16 NR-Multi-RTT-ReportConfig-r16,

additionalPaths-r16 ENUMERATED { requested } OPTIONAL, -- Need ON

...,

[[

nr-UE-RxTxTEG-Request-r17 ENUMERATED { case1, case2, case3, ... }

OPTIONAL, -- Need ON

measureSameDL-PRS-ResourceWithDifferentRxTxTEGs-r17

ENUMERATED { n0, n2, n3, n4, n6, n8, ... }

OPTIONAL, -- Need ON

measureSameDL-PRS-ResourceWithDifferentRxTEGs-r17

ENUMERATED { n0, n2, n3, n4, n6, n8, ... }

OPTIONAL, -- Need ON

reducedDL-PRS-ProcessingSamples-r17

ENUMERATED { requested, ... } OPTIONAL, -- Need ON

nr-los-nlos-IndicatorRequest-r17 SEQUENCE {

type-r17 LOS-NLOS-IndicatorType1-r17,

granularity-r17 LOS-NLOS-IndicatorGranularity1-r17,

...

} OPTIONAL, -- Need ON

additionalPathsExt-r17 ENUMERATED { requested } OPTIONAL, -- Need ON

additionalPathsDL-PRS-RSRP-Request-r17

ENUMERATED { requested } OPTIONAL, -- Need ON

multiMeasInSameReport-r17 ENUMERATED { requested } OPTIONAL, -- Need ON

lowerRxBeamSweepingFactor-FR2-r17 ENUMERATED { requested } OPTIONAL -- Need ON

]],

[[

nr-DL-PRS-RxHoppingRequest-r18 SEQUENCE {

nr-DL-PRS-RxHoppingTotalBandwidth-r18 CHOICE {

fr1 ENUMERATED {mhz40, mhz50, mhz80, mhz100},

fr2 ENUMERATED {mhz100, mhz200, mhz400}

} OPTIONAL -- Need ON

} OPTIONAL, -- Need ON

timingReportingGranularityFactorExt-r18 INTEGER (-6..-1) OPTIONAL, -- Need ON

nr-DL-PRS-JointMeasurementRequest-r18 SEQUENCE {

nr-DL-PRS-JointMeasurementRequestedPFL-List-r18 SEQUENCE (SIZE (2..3)) OF

INTEGER (0..nrMaxFreqLayers-1-r16) OPTIONAL -- Need ON

} OPTIONAL, -- Need ON

nr-DL-PRS-MeasurementTimeWindowsConfig-r18

NR-DL-PRS-MeasurementTimeWindowsConfig-r18 OPTIONAL -- Need ON

]],

[[

nr-NTN-UE-RxTxMeasurementsRequest-r18 ENUMERATED { requested } OPTIONAL -- Need ON

]]

}

NR-Multi-RTT-ReportConfig-r16 ::= SEQUENCE {

maxDL-PRS-RxTxTimeDiffMeasPerTRP-r16 INTEGER (1..4) OPTIONAL, -- Need ON

timingReportingGranularityFactor-r16 INTEGER (0..5) OPTIONAL -- Need ON

}

-- ASN1STOP

|  |
| --- |
| *NR-Multi-RTT-RequestLocationInformation* field descriptions |
| ***nr-UE-RxTxTimeDiffMeasurementInfoRequest***  This field, if present, indicates that the target device is requested to report the DL-PRS Resource ID(s) or DL-PRS Resource Set ID(s) associated with the DL-PRS Resources(s) or the DL-PRS Resource Set(s) which are used in determining the UE Rx-Tx time difference measurements. |
| ***nr-RequestedMeasurements***  This field specifies the NR Multi-RTT measurements requested. This is represented by a bit string, with a one‑value at the bit position means the particular measurement is requested; a zero‑value means not requested. The *dl-PRS-RSCP-Request* means that the target device is requested to provide DL RSCP measurement. |
| ***nr-AssistanceAvailability***  This field indicates whether the target device may request additional DL-PRS assistance data from the server. TRUE means allowed and FALSE means not allowed. |
| ***maxDL-PRS-RxTxTimeDiffMeasPerTRP***  This field specifies the maximum number of UE-Rx-Tx time difference measurements for different DL-PRS Resources or DL-PRS Resource Sets per TRP. |
| ***timingReportingGranularityFactor,*** ***timingReportingGranularityFactorExt***  This field specifies the recommended reporting granularity for the UE Rx-Tx time difference measurements. Value (0..5) corresponds to (*k0*..*k5*) and value (-6..-1) corresponds to (*kMinus6..kMinus1*) used for *nr-UE-RxTxTimeDiff* and *nr-UE-RxTxTimeDiffAdditional* in *NR-Multi-RTT-MeasElement*. The UE may select a different granularity value for *nr-UE-RxTxTimeDiff* and *nr-UE-RxTxTimeDiffAdditional*. The *timingReportingGranularityFactorExt* should not be included by the location server and shall be ignored by the target device if *timingReportingGranularityFactor* is included. The *timingReportingGranularityFactor* should not be included by the location server and shall be ignored by the target device if *timingReportingGranularityFactorExt* is included. |
| ***additionalPaths***  This field, if present, indicates that the target device is requested to provide the *nr-AdditionalPathList* in IE *NR-Multi-RTT-SignalMeasurementInformation*. If this field is present, the field *additionalPathsExt* shall be absent. |
| ***nr-UE-RxTxTEG-Request***  This field, if present, indicates that the target device is requested to provide the *NR-UE-RxTx-TEG-Info* in IE *NR-Multi-RTT-SignalMeasurementInformation.* Enumerated value '*case1*' indicates that the target device is requested to provide the *case1* choice in *NR-UE-RxTx-TEG-Info*, enumerated value '*case2*' indicates that the target device is requested to provide the *case2* choice in *NR-UE-RxTx-TEG-Info*, and so on. |
| ***measureSameDL-PRS-ResourceWithDifferentRxTxTEGs***  This field, if present, indicates that the target device is requested to measure the same DL-PRS Resource of a TRP with *N* different UE RxTx TEGs and with the same UE Tx TEG. Enumerated value '*n0*' indicates that the number *N* of different UE RxTx TEGs to measure the same DL-PRS Resource can be determined by the target device, value '*n2*' indicates that the target device is requested to measure the same DL-PRS Resource of a TRP with 2 different UE RxTx TEGs, value '*n3*' indicates that the target device is requested to measure the same DL-PRS Resource of a TRP with 3 different UE RxTx TEGs, and so on. When the location server requests aggregated measurements, this field indicates a request for configuring the target device to measure the same aggregated DL-PRS Resources of a TRP with N different UE RxTx TEGs.  If this field is present, the field *nr-UE-RxTxTEG-Request* should also be present.  If this field is present, the field *measureSameDL-PRS-ResourceWithDifferentRxTEGs* should not be present. |
| ***measureSameDL-PRS-ResourceWithDifferentRxTEGs***  This field, if present, indicates that the target device is requested to measure the same DL-PRS Resource of a TRP with *N* different UE Rx TEGs. Enumerated value '*n0*' indicates that the number *N* of different UE Rx TEGs to measure the same DL-PRS Resource can be determined by the target device, value '*n2*' indicates that the target device is requested to measure the same DL-PRS Resource of a TRP with 2 different UE Rx TEGs, value '*n3*' indicates that the target device is requested to measure the same DL-PRS Resource of a TRP with 3 different UE Rx TEGs, and so on. When the location server requests aggregated measurements, a request for configuring the UE to measure the same aggregated DL-PRS Resources of a TRP with N different UE Rx TEGs.  If this field is present, the field *nr-UE-RxTxTEG-Request* should also be present.  If this field is present, the field *measureSameDL-PRS-ResourceWithDifferentRxTxTEGs* should not be present. |
| ***reducedDL-PRS-ProcessingSamples***  This field, if present and set to '*requested*', indicates that the target device is requested to perform the requested measurements with reduced number of samples (M=1 or M=2) as specified in TS 38.133 [46]. When requested for aggregated measurements by the location server, this field indicates processing of reduced number of samples for the aggregated measurements. |
| ***nr-los-nlos-IndicatorRequest***  This field, if present, indicates that the target device is requested to provide the indicated type and granularity of the estimated *LOS-NLOS-Indicator* in the *NR-Multi-RTT-SignalMeasurementInformation*. |
| ***additionalPathsExt***  This field, if present, indicates that the target device is requested to provide the *nr-AdditionalPathListExt* in IE *NR-Multi-RTT-SignalMeasurementInformation*. If this field is present, the field *additionalPaths* shall be absent. |
| ***additionalPathsDL-PRS-RSRP-Request***  This field, if present, indicates that the target device is requested to provide the *nr-DL-PRS-RSRPP* for the additional paths in the field *nr-AdditionalPathList* or *nr-AdditionalPathListExt*. |
| ***multiMeasInSameReport***  This field, if present, indicates that the target device is requested to provide multiple measurement instances in a single measurement report; i.e., include the *nr-Multi-RTT-SignalMeasurementInstances* in IE *NR-Multi-RTT-ProvideLocationInformation.* |
| ***lowerRxBeamSweepingFactor-FR2***  This field, if present, indicates that the target device is requested to use a lower Rx beam sweeping factor than 8 for FR2 according to UE's capability. When requested for aggregated measurements by the location server, this field indicates that the target device is requested to use a lower Rx beam sweeping factor than 8 for FR2 according to UE's capability for the aggregated measurements. |
| ***nr-DL-PRS-RxHoppingRequest***  This field, if present, indicates that the target device is requested to use DL-PRS Rx hopping for performing UE-Rx-Tx time difference, RSRP (if requested in *nr-RequestedMeasurements*), or RSRPP measurements (if requested in *nr-RequestedMeasurements*) and report the hopping information used for performing the measurements. This field is not included when *dl-PRS-RSCP-Request* or *nr-DL-PRS-JointMeasurementRequest* is included. |
| ***nr-DL-PRS-RxHoppingTotalBandwidth***  This field, if present, indicates the total bandwidth in MHz across all hops for the DL-PRS measurement. If the configured value *nr-DL-PRS-RxHoppingTotalBandwidth* is larger than the configured DL-PRS bandwidth in the provided assistance data, the UE shall assume that the actual nr-*DL-PRS-RxHoppingTotalBandwidth* is equal to the width of the configured DL-PRS in the provided assistance data. |
| ***nr-DL-PRS-JointMeasurementRequest***  This field, if present, indicates that the target device is requested to perform joint measurement across aggregated PFLs. |
| ***nr-DL-PRS-JointMeasurementRequestedPFL-List***  This field, if present, indicates that the target device is requested to perform joint measurements on the indicated two or three PFLs that are linked for DL-PRS BW aggregation. Value 0 corresponds to the first frequency layer provided in *nr-DL-PRS-AssistanceDataList*, value 1 to the second frequency layer in *nr-DL-PRS-AssistanceDataList*, and so on. |
| ***nr-DL-PRS-MeasurementTimeWindowsConfig***  This field indicates DL-PRS Resource Set(s) occurring within time window(s) for performing measurements where the time window is indicated by a start time, periodicity, offset and duration. |
| ***nr-NTN-UE-RxTxMeasurementsRequest***  This field, if present, indicates that the target device is requested to provide additional measurements for the UE Rx-Tx time difference in NTN, i.e., include *nr-NTN-UE-RxTxMeasurements* in *NR-Multi-RTT-ProvideLocationInformation.* |

#### 6.5.12.6 NR Multi-RTT Capability Information

#### – *NR-Multi-RTT-ProvideCapabilities*

The IE *NR-Multi-RTT-ProvideCapabilities* is used by the target device to indicate its capability to support NR Multi-RTT and to provide its NR Multi-RTT positioning capabilities to the location server.

-- ASN1START

NR-Multi-RTT-ProvideCapabilities-r16 ::= SEQUENCE {

nr-Multi-RTT-PRS-Capability-r16 NR-DL-PRS-ResourcesCapability-r16,

nr-Multi-RTT-MeasurementCapability-r16 NR-Multi-RTT-MeasurementCapability-r16,

nr-DL-PRS-QCL-ProcessingCapability-r16 NR-DL-PRS-QCL-ProcessingCapability-r16,

nr-DL-PRS-ProcessingCapability-r16 NR-DL-PRS-ProcessingCapability-r16,

nr-UL-SRS-Capability-r16 NR-UL-SRS-Capability-r16,

additionalPathsReport-r16 ENUMERATED { supported } OPTIONAL,

periodicalReporting-r16 ENUMERATED { supported } OPTIONAL,

...,

[[

ten-ms-unit-ResponseTime-r17 ENUMERATED { supported } OPTIONAL,

nr-DL-PRS-ExpectedAoD-or-AoA-Sup-r17 BIT STRING { eAoD (0),

eAoA (1)

} (SIZE (1..8)) OPTIONAL, nr-Multi-RTT-On-Demand-DL-PRS-Support-r17

NR-On-Demand-DL-PRS-Support-r17 OPTIONAL,

nr-UE-RxTx-TEG-ID-ReportingSupport-r17 BIT STRING { case1 (0),

case2 (1),

case3 (2)

} (SIZE (1..8)) OPTIONAL,

nr-los-nlos-IndicatorSupport-r17 SEQUENCE {

type-r17 LOS-NLOS-IndicatorType2-r17,

granularity-r17 LOS-NLOS-IndicatorGranularity2-r17,

...

} OPTIONAL,

additionalPathsExtSupport-r17 ENUMERATED { n4, n6, n8 } OPTIONAL,

scheduledLocationRequestSupported-r17 ScheduledLocationTimeSupport-r17 OPTIONAL,

nr-dl-prs-AssistanceDataValidity-r17 SEQUENCE {

area-validity-r17 INTEGER (1..maxNrOfAreas-r17) OPTIONAL,

...

} OPTIONAL,

multiMeasInSameMeasReport-r17 ENUMERATED { supported } OPTIONAL,

mg-ActivationRequest-r17 ENUMERATED { supported } OPTIONAL

]],

[[

posMeasGapSupport-r17 ENUMERATED { supported } OPTIONAL

]],

[[

nr-MultiRTT-OnDemandPRS-ForBWA-Support-r18 ENUMERATED { supported } OPTIONAL,

periodicReportingIntervalMsSupport-r18 PeriodicReportingIntervalMsSupport-r18 OPTIONAL

]]

}

-- ASN1STOP

| *NR-Multi-RTT-ProvideCapabilities* field descriptions |
| --- |
| ***ten-ms-unit-ResponseTime***  This field, if present, indicates that the target device supports the enumerated value '*ten-milli-seconds*' in the IE *ResponseTime* in IE *CommonIEsRequestLocationInformation*. |
| ***nr-DL-PRS-ExpectedAoD-or-AoA-Sup***  This field, if present, indicates that the target device supports the *NR-DL-PRS-ExpectedAoD-or-AoA* in *NR-DL-PRS-AssistanceData.* |
| ***nr-Multi-RTT-On-Demand-DL-PRS-Support***  This field, if present, indicates that the target device supports on-demand DL-PRS requests. |
| ***nr-UE-RxTx-TEG-ID-ReportingSupport***  This field, if present, indicates that the target device supports *nr-UE-RxTx-TEG-Info* reporting in IE *NR-Multi-RTT-SignalMeasurementInformation.* This is represented by a bit string, with a one‑value at the bit position means the particular case is supported; a zero‑value means not supported:  - bit 0indicates that the target device supports the '*case1*' choice in *NR-UE-RxTx-TEG-Info*.  - bit 1 indicates that the target device supports the '*case2*' choice in *NR-UE-RxTx-TEG-Info*.  - bit 2 indicates that the target device supports the '*case3*' choice in *NR-UE-RxTx-TEG-Info*. |
| ***nr-los-nlos-IndicatorSupport***  This field, if present, indicates that the target device supports *nr-los-nlos-Indicator* reporting in IE *NR-Multi-RTT-SignalMeasurementInformation*.  - *type* indicates whether the target device supports '*hard*' value or '*hard*' and '*soft*' value in IE *LOS-NLOS-Indicator.*  - *granularity* indicates whether the target device supports *LOS-NLOS-Indicator* reporting per TRP, per DL-PRS Resource, or both.  NOTE: A single value is reported when both Multi-RTT and DL-TDOA are supported. |
| ***additionalPathsExtSupport***  This field, if present, indicates that the target device supports the *nr-AdditionalPathListExt* reporting in IE *NR-Multi-RTT-SignalMeasurementInformation*. The enumerated value indicates the number of additional paths supported by the target device.  NOTE: The *supportOfDL-PRS-FirstPathRSRP* in IE *NR-Multi-RTT-MeasurementCapability* also applies to the additional paths. |
| ***scheduledLocationRequestSupported***  This field, if present, indicates that the target device supports scheduled location requests – i.e., supports the IE *ScheduledLocationTime* in IE *CommonIEsRequestLocationInformation* – and the time base(s) supported for the scheduled location time. |
| ***nr-dl-prs-AssistanceDataValidity***  This field, if present, indicates that the target device supports validity conditions for pre-configured assistance data and comprises the following subfields:  - ***area-validity*** indicates that the target device supports pre-configured assistance data with area validity. The integer number indicates the maximum number of areas the target device supports*.* |
| ***multiMeasInSameMeasReport***  This field, if present, indicates that the target device supports multiple measurement instances in a single measurement report. |
| ***mg-ActivationRequest***  This field, if present, indicates that the target device supports UL MAC CE for positioning measurement gap activation/deactivation request for DL-PRS measurements. The UE can include this field only if the UE supports *mg-ActivationRequestPRS-Meas* and *mg-ActivationCommPRS-Meas* defined in TS 38.331 [35]. |
| ***posMeasGapSupport***  This field, if present, indicates that the target device supports pre-configured positioning measurement gap for DL-PRS measurements. The UE can include this field only if the UE supports *mg-ActivationCommPRS-Meas* defined in TS 38.331 [35]. |
| ***nr-MultiRTT-OnDemandPRS-ForBWA-Support***  This field, if present, indicates that the target device supports on-demand DL-PRS request for bandwidth aggregation. |
| ***periodicReportingIntervalMsSupport***  This field, if present, indicates that the target device supports millisecond periodic reporting intervals for location information – i.e., supports the subfield *reportingIntervalMs* of the IE *PeriodicalReportingCriteriaExt* in IE *CommonIEsRequestLocationInformation* – and the minimum millisecond report interval supported for the periodic reporting. |

#### 6.5.12.6a NR Multi-RTT Capability Information Elements

#### *– NR-Multi-RTT-MeasurementCapability*

The IE *NR-Multi-RTT-MeasurementCapability* defines the Multi-RTT measurement capability. The UE can include this IE only if the UE supports *NR-DL-PRS-ResourcesCapability* for Multi-RTT. Otherwise, the UE does not include this IE;

-- ASN1START

NR-Multi-RTT-MeasurementCapability-r16 ::= SEQUENCE {

maxNrOfRx-TX-MeasFR1-r16 INTEGER (1..4) OPTIONAL,

maxNrOfRx-TX-MeasFR2-r16 INTEGER (1..4) OPTIONAL,

supportOfRSRP-MeasFR1-r16 ENUMERATED { supported } OPTIONAL,

supportOfRSRP-MeasFR2-r16 ENUMERATED { supported } OPTIONAL,

srs-AssocPRS-MultiLayersFR1-r16 ENUMERATED { supported } OPTIONAL,

srs-AssocPRS-MultiLayersFR2-r16 ENUMERATED { supported } OPTIONAL,

...,

[[

nr-UE-TEG-Capability-r17 NR-UE-TEG-Capability-r17 OPTIONAL,

multi-RTT-MeasCapabilityBandList-r17 SEQUENCE (SIZE (1..nrMaxBands-r16)) OF

Multi-RTT-MeasCapabilityPerBand-r17

OPTIONAL

]]

}

Multi-RTT-MeasCapabilityPerBand-r17 ::= SEQUENCE {

freqBandIndicatorNR-r17 FreqBandIndicatorNR-r16,

supportOfDL-PRS-FirstPathRSRP-r17 ENUMERATED { supported } OPTIONAL,

dl-PRS-MeasRRC-Inactive-r17 ENUMERATED { supported } OPTIONAL,

...,

[[

supportOfDL-PRS-BWA-RRC-Connected-r18 ENUMERATED { supported } OPTIONAL,

supportOfDL-PRS-BWA-RRC-Inactive-r18 ENUMERATED { supported } OPTIONAL,

nr-NTN-MeasAndReport-r18 ENUMERATED { supported } OPTIONAL,

nr-DL-PRS-RSCP-RRC-Connected-r18 ENUMERATED { supported } OPTIONAL,

nr-DL-PRS-RSCP-RRC-Inactive-r18 ENUMERATED { supported } OPTIONAL,

assocSingleRx-Tx-WithUpToNsampleRSCP-r18 ENUMERATED { supported } OPTIONAL,

supportOfSymbolTimeStampForRSCP-r18 ENUMERATED { supported } OPTIONAL,

supportOfFinerTimingReportGranularityForPRS-Meas-r18 ENUMERATED { minus1, minus2,

minus3, minus4, minus5, minus6} OPTIONAL,

supportOfMeasurementsInTimeWindow-r18 BIT STRING { rx-tx (0),

rsrp (1),

rsrpp (2),

rscp (3)

} (SIZE (1..8)) OPTIONAL

]]

}

-- ASN1STOP

|  |
| --- |
| *NR-Multi-RTT-MeasurementCapability* field descriptions |
| ***maxNrOfRx-TX-MeasFR1***  Indicates the maximum number of UE Rx–Tx time difference measurements corresponding to a single SRS resource/resource set for positioning with each measurement corresponding to a single DL-PRS Resource/Resource Set on FR1. |
| ***maxNrOfRx-TX-MeasFR2***  Indicates the maximum number of UE Rx–Tx time difference measurements corresponding to a single SRS resource/resource set for positioning with each measurement corresponding to a single DL-PRS Resource/Resource Set on FR2. |
| ***srs-AssocPRS-MultiLayersFR1***  Indicates whether the UE supports measurements derived on one or more DL-PRS Resource/Resource Sets which may be in different positioning frequency layers for SRS transmitted in a single CC. DL-PRS and SRS may be on different bands. This is for FR1 only. |
| ***srs-AssocPRS-MultiLayersFR2***  Indicates whether the UE supports measurements derived on one or more DL-PRS Resource/Resource Sets which may be in different positioning frequency layers for SRS transmitted in a single CC. DL-PRS and SRS may be on different bands. This is for FR2 only. |
| ***supportOfRSRP-MeasFR1***  Indicates whether the UE supports RSRP measurement for Multi-RTT on FR1. |
| ***supportOfRSRP-MeasFR2***  Indicates whether the UE supports RSRP measurement for Multi-RTT on FR2. |
| ***nr-UE-TEG-Capability***  Indicates the UE TEG capability. |
| ***supportOfDL-PRS-FirstPathRSRP***  Indicates whether the target device supports DL-PRS RSRPP of first path measurement for Multi-RTT. The UE can include this field only if the UE supports *prs-ProcessingCapabilityBandList*. Otherwise, the UE does not include this field. The UE supporting *additionalPathsReport* and *supportOfDL-PRS-FirstPathRSRP* shall support RSRPP reporting for K=1 or 2 additional paths. |
| ***dl-PRS-MeasRRC-Inactive***  This field, if present, indicates that the target device supports DL-PRS measurement in RRC\_INACTIVE state. The UE can include this field only if the UE supports *maxNrOfDL-PRS-ResourceSetPerTrpPerFrequencyLayer, maxNrOfTRP-AcrossFreqs, maxNrOfPosLayer* and *dl-PRS-BufferType-RRC-Inactive*. Otherwise, the UE does not include this field.  NOTE 1: The capabilities *NR-DL-PRS-ResourcesCapability, maxNrOfRx-TX-MeasFR1, maxNrOfRx-TX-MeasFR2, supportOfRSRP-MeasFR1, supportOfRSRP-MeasFR2, srs-AssocPRS-MultiLayersFR1, srs-AssocPRS-MultiLayersFR2, simul-NR-DL-AoD-Multi-RTT* are the same in RRC\_INACTIVE state. |
| ***supportOfDL-PRS-BWA-RRC-Connected***  Indicates whether the target device supports DL-PRS bandwidth aggregation in RRC\_CONNECTED for Multi-RTT. The target device can include this field only if the target device supports *maxNrOfDL-PRS-ResourceSetPerTrpPerFrequencyLayer*, *maxNrOfTRP-AcrossFreqs*, *maxNrOfPosLayer* and *prs-BWA-TwoContiguousIntrabandInMG-RRC-Connected*. Otherwise, the UE does not include this field. |
| ***supportOfDL-PRS-BWA-RRC-Inactive***  Indicates whether the target device supports DL-PRS bandwidth aggregation in RRC\_INACTIVE for Multi-RTT. The target device can include this field only if the target device supports *dl-PRS-MeasRRC-Inactive* and *prs-BWA-TwoContiguousIntraband-RRC-IdleandInactive*. Otherwise, the target device does not include this field. |
| ***nr-NTN-MeasAndReport***  This field, if present, indicates that the UE supports UE Rx-Tx Measurement and Report for Multi-RTT with single satellite in NTN with the following capabilities:  - UE Rx-Tx time difference based on single sample and UE Rx-Tx time difference offset measurement and report for Multi-RTT positioning;  - Reporting DL timing drift due to Doppler over the service link associated with the UE Rx-Tx time difference measurement period.  NOTE 2: This field is only present, if *freqBandIndicatorNR* indicates the bands in Table 5.2.2-1 and Table 5.2.3-1 in TS 38.101-5 [54]. |
| ***nr-DL-PRS-RSCP-RRC-Connected***  This field, if present, indicates that the target device supports DL RSCP measurements in RRC\_CONNECTED. The UE can include this field only if the UE supports *maxNrOfRx-TX-MeasFR1, maxNrOfRx-TX-MeasFR2, supportOfRSRP-MeasFR1* and *supportOfRSRP-MeasFR2*. Otherwise, the UE does not include this field.  NOTE 3: RSCP is reported together with UE Rx-Tx time difference measurement. |
| ***nr-DL-PRS-RSCP-RRC-Inactive***  This field, if present, indicates that the target device supports DL RSCP measurements in RRC\_INACTIVE. The UE can include this field only if the UE supports *dl-PRS-MeasRRC-Inactive*. Otherwise, the UE does not include this field.  NOTE 4: RSCP is reported together with UE Rx-Tx time difference measurement. |
| ***assocSingleRx-Tx-WithUpToNsampleRSCP***  This field, if present, indicates that the target device supports associating a single Rx-Tx measurement with up to N\_sample RSCP measurement. The UE can include this field only if the UE supports one of *nr-DL-PRS-RSCP-RRC-Connected* and *nr-DL-PRS-RSCP-RRC-Inactive*. Otherwise, the UE does not include this field. |
| ***supportOfSymbolTimeStampForRSCP***  This field, if present, indicates that the target device supports reporting timestamp with OFDM symbol index associated with RSCP measurement. The UE can include this field only if the UE supports one of *nr-DL-PRS-RSCP-RRC-Connected* and *nr-DL-PRS-RSCP-RRC-Inactive*. Otherwise, the UE does not include this field. |
| ***supportOfFinerTimingReportGranularityForPRS-Meas***  This field, if present, indicates that the target device supports finer timing reporting granularity for DL-PRS measurement. |
| ***supportOfMeasurementsInTimeWindow***  This field, if present, indicates that the target device supports performing measurements inside the indicated time window only for Multi-RTT. This is represented by a bit string, with a one‑value at the bit position means the particular measurement is supported; a zero‑value means not supported.  - bit 0 indicates whether performing UE Rx-Tx time difference is supported or not;  - bit 1 indicates whether performing DL PRS-RSRP is supported or not;  - bit 2 indicates whether performing DL PRS-RSRPP is supported or not;  - bit 3 indicates whether performing DL PRS-RSCP is supported or not;  The UE can include this field only if the UE supports *maxNrOfDL-PRS-ResourcesPerResourceSet* and *maxNrOfDL-PRS-ResourcesPerPositioningFrequencylayer*. Otherwise, the UE does not include this field. |

#### 6.5.12.7 NR Multi-RTT Capability Information Request

#### – *NR-Multi-RTT-RequestCapabilities*

The IE *NR-Multi-RTT-RequestCapabilities* is used by the location server to request the capability of the target device to support NR Multi-RTT and to request NR Multi-RTT positioning capabilities from a target device.

-- ASN1START

NR-Multi-RTT-RequestCapabilities-r16 ::= SEQUENCE {

...

}

-- ASN1STOP

#### 6.5.12.8 NR Multi-RTT Error Elements

#### – *NR-Multi-RTT-Error*

The IE *NR-Multi-RTT-Error* is used by the location server or target device to provide NR Multi-RTT error reasons to the target device or location server, respectively.

-- ASN1START

NR-Multi-RTT-Error-r16 ::= CHOICE {

locationServerErrorCauses-r16 NR-Multi-RTT-LocationServerErrorCauses-r16,

targetDeviceErrorCauses-r16 NR-Multi-RTT-TargetDeviceErrorCauses-r16,

...

}

-- ASN1STOP

#### – *NR-Multi-RTT-LocationServerErrorCauses*

The IE *NR-Multi-RTT-LocationServerErrorCauses* is used by the location server to provide NR Multi-RTT error reasons to the target device.

-- ASN1START

NR-Multi-RTT-LocationServerErrorCauses-r16 ::= SEQUENCE {

cause-r16 ENUMERATED { undefined,

assistanceDataNotSupportedByServer,

assistanceDataSupportedButCurrentlyNotAvailableByServer,

...,

on-demand-dl-prs-NotSupportedByServer-v1700,

on-demand-dl-prs-SupportedButCurrentlyNotAvailableByServer-v1700

},

...

}

-- ASN1STOP

#### – *NR-Multi-RTT-TargetDeviceErrorCauses*

The IE *NR-Multi-RTT-TargetDeviceErrorCauses* is used by the target device to provide NR Multi-RTT error reasons to the location server.

-- ASN1START

NR-Multi-RTT-TargetDeviceErrorCauses-r16 ::= SEQUENCE {

cause-r16 ENUMERATED { undefined,

dl-assistance-data-missing,

unableToMeasureAnyTRP,

attemptedButUnableToMeasureSomeNeighbourTRPs,

ul-srs-configuration-missing,

unableToTransmit-ul-srs,

...

},

...,

[[

remoteUE-Indication-r18 ENUMERATED {true} OPTIONAL -- Cond NR

]]

}

-- ASN1STOP

| Conditional presence | Explanation |
| --- | --- |
| *NR* | This field is optionally present, need OR, for NR access. Otherwise it is not present. |

| *NR-Multi-RTT-TargetDeviceErrorCauses* field descriptions |
| --- |
| ***remoteUE-Indication***  This field indicates whether the target device in NR access is configured as a L2 U2N Remote UE. |

### 6.5.13 NR AI/ML Positioning

This clause defines the information elements for NR AI/ML direct positioning (TS 38.305 [40]).

#### 6.5.13.1 NR AI/ML Positioning Assistance Data

#### – *NR-AI-ML-PositioningProvideAssistanceData*

The IE *NR-AI-ML-PositioningProvideAssistanceData* is used by the location server to provide assistance data to enable UE-based AI/ML direct positioning. It may also be used to provide NR AI/ML positioning specific error reason.

-- ASN1START

NR-AI-ML-PositioningProvideAssistanceData-r19 ::= SEQUENCE {

nr-DL-PRS-AssistanceData-r19 NR-DL-PRS-AssistanceData-r16 OPTIONAL, -- Need ON

nr-SelectedDL-PRS-IndexList-r19 NR-SelectedDL-PRS-IndexList-r16 OPTIONAL, -- Need ON

nr-On-Demand-DL-PRS-Configurations-r19

NR-On-Demand-DL-PRS-Configurations-r17

OPTIONAL, -- Need ON

nr-On-Demand-DL-PRS-Configurations-Selected-IndexList-r19

NR-On-Demand-DL-PRS-Configurations-Selected-IndexList-r17 OPTIONAL, -- Need ON

assistanceDataValidityArea-r19 AreaID-CellList-r17 OPTIONAL, -- Need ON

nr-PositionCalculationAssistance-r19

NR-PositionCalculationAssistance-r16

OPTIONAL, -- Need ON

nr-AI-ML-Positioning-Error-r19 NR-AI-ML-Positioning-Error-r19 OPTIONAL, -- Need ON

...

}

-- ASN1STOP

Editor's Note: The above list of assistance data elements is FFS and depends on further RAN1/RAN2 agreements. The draft list above is the same as in IE *NR-DL-TDOA-ProvideAssistanceData* but without the *NR-PeriodicAssistData.*

|  |
| --- |
| *NR-AI-ML-PositioningProvideAssistanceData* field descriptions |
| ***nr-DL-PRS-AssistanceData***  This field specifies the assistance data reference and neighbour TRPs and provides the DL-PRS configuration for the TRPs.  Note, if this field is absent but the *nr-SelectedDL-PRS-IndexList* field is present, the *nr-DL-PRS-AssistanceData* may be provided in IE *NR-DL-TDOA-ProvideAssistanceData* or *NR-DL-AoD-ProvideAssistanceData*. |
| ***nr-SelectedDL-PRS-IndexList***  This field specifies the DL-PRS Resources which are applicable for this *NR-AI-ML-PositioningProvideAssistanceData* message. |
| ***nr-On-Demand-DL-PRS-Configurations***  This field provides a set of available DL-PRS configurations which can be requested by the target device on-demand.  NOTE: If this field is absent but the *nr-On-Demand-DL-PRS-Configurations-Selected-IndexList* is present, the *nr-On-Demand-DL-PRS-Configurations* may be provided in IE *NR-DL-TDOA-ProvideAssistanceData* or *NR-DL-AoD-ProvideAssistanceData*. |
| ***nr-On-Demand-DL-PRS-Configurations-Selected-IndexList***  This field specifies the selected available on-demand DL-PRS configurations which are applicable for this *NR-AI-ML-PositioningProvideAssistanceData message*. |
| ***assistanceDataValidityArea***  This field specifies the network area for which this *NR-AI-ML-PositioningProvideAssistanceData* is valid. |
| ***nr-PositionCalculationAssistance***  This field provides the position calculation assistance data. |
| ***nr-AI-ML-Positioning-Error***  This field provides AI/ML positioning error reasons. |

#### 6.5.13.2 NR AI/ML Positioning Assistance Data Request

#### – *NR-AI-ML-PositioningRequestAssistanceData*

The IE *NR-AI-ML-PositioningRequestAssistanceData* is used by the target device to request assistance data from a location server for NR AI/ML direct positioning.

-- ASN1START

NR-AI-ML-PositioningRequestAssistanceData-r19 ::= SEQUENCE {

nr-PhysCellID-r19 NR-PhysCellID-r16 OPTIONAL,

nr-DL-PRS-AssistanceDataReq-r19 ENUMERATED { requested } OPTIONAL,

nr-DL-PRS-ExpectedAoD-or-AoA-Req-r19 ENUMERATED { eAoD, eAoA } OPTIONAL,

nr-on-demand-DL-PRS-Req-r19 NR-On-Demand-DL-PRS-Request-r17 OPTIONAL,

pre-configured-AssistanceDataReq-r19 ENUMERATED { true } OPTIONAL,

nr-PositionCalculationAssistanceReq-r19 BIT STRING {

trpLoc (0),

beamInfo (1),

rtdInfo (2),

losNlosInfo (3),

trpTEG-Info (4),

nr-IntegrityBounds (5),

pruInfo (6)

} (SIZE (1..8)) OPTIONAL,

nr-IntegrityAssistanceReq-r19 BIT STRING {

serviceParameters (0),

serviceAlert (1),

riskParameters (2),

integrityParaTRP-Loc (3),

integrityParaBeamInfo (4),

integrityParaRTD-Info (5)

} (SIZE (1..8)) OPTIONAL,

...

}

-- ASN1STOP

Editor's Note: The above list of assistance data request elements is FFS and depends on further RAN1/RAN2 agreements. The list above is based on IE *NR-AI-ML-PositioningProvideAssistanceData* (*NR-DL-TDOA-RequestAssistanceData*)*.*

|  |
| --- |
| *NR-AI-ML-PositioningRequestAssistanceData* field descriptions |
| ***nr-PhysCellID***  This field specifies the NR physical cell identity of the current primary cell of the target device. |
| ***nr-DL-PRS-AssistanceDataReq***  This field, if present, indicates that the *nr-DL-PRS-AssistanceData* are requested. |
| ***nr-DL-PRS-ExpectedAoD-or-AoA-Req***  This field, if present, indicates that the IE *NR-DL-PRS-ExpectedAoD-or-AoA* in *NR-DL-PRS-AssistanceData* is requested. Enumerated value '*eAoD*' indicates that expected AoD information is requested; value '*eAoA*' indicates that expected AoA information is requested. |
| ***nr-on-demand-DL-PRS-Req***  This field indicates the on-demand DL-PRS requested for AI/ML direct positioning. |
| ***pre-configured-AssistanceDataReq***  This field, if present, indicates that the target device requests pre-configured assistance data with area validity. |
| ***nr-PositionCalculationAssistanceReq***  This field indicates the Position Calculation Assistance Data requested. This is represented by a bit string, with a one‑value at the bit position means the particular assistance data is requested; a zero‑value means not requested.  - bit 0 indicates whether the field *nr-TRP-LocationInfo* in IE *NR-PositionCalculationAssistance* is requested or not;  - bit 1 indicates whether the field *nr-DL-PRS-BeamInfo* in IE *NR-PositionCalculationAssistance* is requested or not;  - bit 2 indicates whether the field *nr-RTD-Info* in IE *NR-PositionCalculationAssistance* is requested or not;  - bit 3 indicates whether the field *nr-DL-PRS-Expected-LOS-NLOS-Assistance* in IE *NR-PositionCalculationAssistance* is requested or not;  - bit 4 indicates whether the field *nr-DL-PRS-TRP-TEG-Info* in IE *NR-PositionCalculationAssistance* is requested or not;  - bit 5 together with bit 0 indicates whether the fields *nr-IntegrityTRP-LocationBounds*, *nr-IntegrityDL-PRS-ResourceSetARP-LocationBounds*, *nr-IntegrityDL-PRS-ResourceARP-LocationBounds* in IE *NR-TRP-LocationInfo* are requested or not; bit 5 together with bit 1 indicates whether the field *nr-IntegrityBeamInfoBounds* in IE *NR-DL-PRS-BeamInfo* is requested or not; bit 5 together with the bit 2 indicates whether the field *nr-IntegrityRTD-InfoBounds* in IE *NR-RTD-Info* is requested or not;  - bit 6 indicates whether the field *nr-PRU-DL-Info* in IE *NR-PositionCalculationAssistance* is requested or not. |
| ***nr-IntegrityAssistanceReq***  This field indicates the Integrity Assistance Data requested. This is represented by a bit string, with a one‑value at the bit position means the particular assistance data is requested; a zero‑value means not requested.  - bit 0 indicates whether the field *nr-IntegrityServiceParameters* in IE *NR-PositionCalculationAssistance* is requested or not;  - bit 1 indicates whether the field *nr-IntegrityServiceAlert* in IE *NR-PositionCalculationAssistance* is requested or not;  - bit 2 indicates whether the field *nr-IntegrityRiskParameters* in IE *NR-PositionCalculationAssistance* is requested or not;  - bit 3 indicates whether the field *nr-IntegrityParametersTRP-LocationInfo* in IE *NR-PositionCalculationAssistance* is requested or not;  - bit 4 indicates whether the field *nr-IntegrityParametersDL-PRS-BeamInfo* in IE *NR-PositionCalculationAssistance* is requested or not;  - bit 5 indicates whether the field *nr-IntegrityParametersRTD-Info* in IE *NR-PositionCalculationAssistance* is requested or not. |

#### 6.5.13.3 NR AI/ML Positioning Location Information

#### – *NR-AI-ML-PositioningProvideLocationInformation*

The IE *NR-AI-ML-PositioningProvideLocationInformation* is used by the target device to provide NR AI/ML location information to the location server. It may also be used to provide NR AI/ML positioning specific error reason.

-- ASN1START

NR-AI-ML-PositioningProvideLocationInformation-r19 ::= SEQUENCE {

nr-AI-ML-LocationInformation-r19 NR-AI-ML-LocationInformation-r19 OPTIONAL,

nr-AI-ML-LocationInformationInstances-r19 SEQUENCE (SIZE (1..maxMeasInstances-r17)) OF

NR-AI-ML-LocationInformation-r19

OPTIONAL, -- Cond batch

nr-AI-ML-Positioning-Error-r19 NR-AI-ML-Positioning-Error-r19 OPTIONAL,

...

}

-- ASN1STOP

| Conditional presence | Explanation |
| --- | --- |
| *batch* | The field is optionally present if the field *nr-AI-ML-LocationInformation* is absent; otherwise it is not present. |

Editor's Note: FFS whether batch reporting is also applicable to AI/ML positioning.

#### 6.5.13.4 NR AI/ML Positioning Location Information Elements

#### *– NR-AI-ML-LocationInformation*

The IE *NR-AI-ML-LocationInformation* is included by the target device when location information derived by using NR AI/ML is provided to the location server.

-- ASN1START

NR-AI-ML-LocationInformation-r19 ::= SEQUENCE {

measurementReferenceTime-r19 CHOICE {

systemFrameNumber-r19 NR-TimeStamp-r16,

utc-time-r19 UTCTime,

...

} OPTIONAL,

...

}

-- ASN1STOP

Editor's Note: FFS on information provided in *NR-AI-ML-LocationInformation*.

|  |
| --- |
| *NR-AI-ML-LocationInformation* field descriptions |
| ***measurementReferenceTime***  This field specifies the time for which the location estimate is valid. |

#### 6.5.13.5 NR AI/ML Positioning Location Information Request

#### – *NR-AI-ML-PositioningRequestLocationInformation*

The IE *NR-AI-ML-PositioningRequestLocationInformation* is used by the location server to request NR AI/ML location information from a target device using direct AI/ML positioning.

-- ASN1START

NR-AI-ML-PositioningRequestLocationInformation-r19 ::= SEQUENCE {

nr-AssistanceAvailability-r19 BOOLEAN,

...

}

-- ASN1STOP

Editor's Note: FFS on information included in *NR-AI-ML-PositioningRequestLocationInformation*.

|  |
| --- |
| *NR-AI-ML-PositioningRequestLocationInformation* field descriptions |
| ***nr-AssistanceAvailability***  This field indicates whether the target device may request additional assistance data from the server. TRUE means allowed and FALSE means not allowed. |

#### 6.5.13.6 NR AI/ML Positioning Capability Information

#### – *NR-AI-ML-PositioningProvideCapabilities*

The IE *NR-AI-ML-PositioningProvideCapabilities* is used by the target device to indicate its capability to support NR AI/ML direct positioning and to provide its NR AI/ML positioning capabilities to the location server.

-- ASN1START

NR-AI-ML-PositioningProvideCapabilities-r19 ::= SEQUENCE {

locationCoordinateTypes-r19 LocationCoordinateTypes OPTIONAL,

periodicalReporting-r19 ENUMERATED { supported } OPTIONAL,

periodicReportingIntervalMsSupport-r19 PeriodicReportingIntervalMsSupport-r18 OPTIONAL,

ten-ms-unit-ResponseTime-r19 ENUMERATED { supported } OPTIONAL,

scheduledLocationRequestSupported-r19 ScheduledLocationTimeSupport-r17 OPTIONAL,

nr-PosCalcAssistanceSupport-r19 BIT STRING {

trpLocSup (0),

beamInfoSup (1),

rtdInfoSup (2),

trpTEG-InfoSup (3),

nr-IntegritySup (4),

pruInfoSup (5)

} (SIZE (1..8)) OPTIONAL,

nr-los-nlos-AssistanceDataSupport-r19 SEQUENCE {

type LOS-NLOS-IndicatorType2-r17,

granularity LOS-NLOS-IndicatorGranularity2-r17,

...

} OPTIONAL,

nr-DL-PRS-ExpectedAoD-or-AoA-Sup-r19 BIT STRING {

eAoD (0),

eAoA (1)

} (SIZE (1..8)) OPTIONAL,

nr-On-Demand-DL-PRS-Support-r19 NR-On-Demand-DL-PRS-Support-r17 OPTIONAL,

nr-OnDemandPRS-ForBWA-Support-r19 ENUMERATED { supported } OPTIONAL,

nr-dl-prs-AssistanceDataValidity-r19 SEQUENCE {

area-validity INTEGER (1..maxNrOfAreas-r17) OPTIONAL,

...

} OPTIONAL,

multiLocationEstimateInSameMeasReport-r19 ENUMERATED { supported } OPTIONAL,

nr-IntegrityAssistanceSupport-r19 BIT STRING {

serviceParametersSup (0),

serviceAlertSup (1),

riskParametersSup (2),

integrityParaTRP-LocSup (3),

integrityParaBeamInfoSup (4),

integrityParaRTD-InfoSup (5)

} (SIZE (1..8)) OPTIONAL,

...

}

-- ASN1STOP

Editor's Note: The above list of capability elements is FFS and depends on further RAN1/RAN2 agreements. The list above includes the common LPP capabilities and assistance data supported (per *NR-AI-ML-PositioningProvideAssistanceData* (*NR-DL-TDOA-ProvideAssistanceData*))*.* DL-PRS capabilities are not yet included above.

|  |
| --- |
| *NR-AI-ML-PositioningProvideCapabilities* field descriptions |
| ***locationCoordinateTypes***  This field indicates the geographical location coordinate types that a target device supports for AI/ML direct positioning. TRUE indicates that a location coordinate type is supported and FALSE that it is not. |
| ***periodicalReporting***  This field, if present, indicates that the target device supports *periodicalReporting.* If this field is absent, the target device does not support *periodicalReporting* in *CommonIEsRequestLocationInformation*. |
| ***periodicReportingIntervalMsSupport***  This field, if present, indicates that the target device supports the *reportingIntervalMs* in IE *PeriodicalReportingCriteriaExt* in IE *CommonIEsRequestLocationInformation* and specifies the minimum millisecond periodic reporting interval supported. |
| ***ten-ms-unit-ResponseTime***  This field, if present, indicates that the target device supports the enumerated value '*ten-milli-seconds*' in the IE *ResponseTime* in IE *CommonIEsRequestLocationInformation*. |
| ***scheduledLocationRequestSupported***  This field, if present, indicates that the target device supports scheduled location requests – i.e., supports the IE *ScheduledLocationTime* in IE *CommonIEsRequestLocationInformation* – and the time base(s) supported for the scheduled location time. |
| ***nr-PosCalcAssistanceSupport***  This field indicates the Position Calculation Assistance Data supported by the target device. This is represented by a bit string, with a one‑value at the bit position means the particular assistance data is supported; a zero‑value means not supported.  - bit 0 indicates whether the field *nr-TRP-LocationInfo* in IE *NR-PositionCalculationAssistance* is supported or not;  - bit 1 indicates whether the field *nr-DL-PRS-BeamInfo* in IE *NR-PositionCalculationAssistance* is supported or not;  - bit 2 indicates whether the field *nr-RTD-Info* in IE *NR-PositionCalculationAssistance* is supported or not;  - bit 3 indicates whether the field *nr-DL-PRS-TRP-TEG-Info* in IE *NR-PositionCalculationAssistance* is supported or not;  - bit 4 together with bit 0 indicates whether the fields *nr-IntegrityTRP-LocationBounds*, *nr-IntegrityDL-PRS-ResourceSetARP-LocationBounds*, *nr-IntegrityDL-PRS-ResourceARP-LocationBounds* in IE *NR-TRP-LocationInfo* are supported or not; bit 4 together with bit 1 indicates whether the field *nr-IntegrityBeamInfoBounds* in IE *NR-DL-PRS-BeamInfo* is supported or not; bit 4 together with the bit 2 indicates whether the field *nr-IntegrityRTD-InfoBounds* in IE *NR-RTD-Info* is supported or not;  - bit 5 indicates whether the field *nr-PRU-DL-Info* in IE *NR-PositionCalculationAssistance* is supported or not. |
| ***nr-los-nlos-AssistanceDataSupport***  This field, if present, indicates that the target device supports the *NR-DL-PRS-ExpectedLOS-NLOS-Assistance* in IE *NR-PositionCalculationAssistance*:  - *type* indicates whether the target device supports '*hard*' value or '*hard*' and '*soft*' value in *LOS-NLOS-Indicator* in IE *NR-DL-PRS-ExpectedLOS-NLOS-Assistance*.  - *granularity* indicates whether the target device supports *nr-los-nlos-indicator* in IE *NR-DL-PRS-ExpectedLOS-NLOS-Assistance* '*per-trp*', '*per-resource*', or both. |
| ***nr-DL-PRS-ExpectedAoD-or-AoA-Sup***  This field, if present, indicates that the target device supports the *NR-DL-PRS-ExpectedAoD-or-AoA* in *NR-DL-PRS-AssistanceData.* |
| ***nr-On-Demand-DL-PRS-Support***  This field, if present, indicates that the target device supports on-demand DL-PRS requests. |
| ***nr-OnDemandPRS-ForBWA-Support***  This field, if present, indicates that the target device supports on-demand DL-PRS request for bandwidth aggregation. |
| ***nr-dl-prs-AssistanceDataValidity***  This field, if present, indicates that the target device supports validity conditions for pre-configured assistance data and comprises the following subfields:  - ***area-validity*** indicates that the target device supports pre-configured assistance data with area validity. The integer number indicates the maximum number of areas the target device supports*.* |
| ***multiLocationEstimateInSameMeasReport***  This field, if present, indicates that the target device supports multiple location estimate instances in a single measurement report. |
| ***nr-IntegrityAssistanceSupport***  This field indicates the Integrity Assistance Data supported. This is represented by a bit string, with a one‑value at the bit position means the particular assistance data is supported; a zero‑value means not supported.  - bit 0 indicates whether the field *nr-IntegrityServiceParameters* in IE *NR-PositionCalculationAssistance* is supported or not;  - bit 1 indicates whether the field *nr-IntegrityServiceAlert* in IE *NR-PositionCalculationAssistance* is supported or not;  - bit 2 indicates whether the field *nr-IntegrityRiskParameters* in IE *NR-PositionCalculationAssistance* is supported or not;  - bit 3 indicates whether the field *nr-IntegrityParametersTRP-LocationInfo* in IE *NR-PositionCalculationAssistance* is supported or not;  - bit 4 indicates whether the field *nr-IntegrityParametersDL-PRS-BeamInfo* in IE *NR-PositionCalculationAssistance* is supported or not;  - bit 5 indicates whether the field *nr-IntegrityParametersRTD-Info* in IE *NR-PositionCalculationAssistance* is supported or not. |

#### 6.5.13.7 NR AI/ML Positioning Capability Information Request

#### – *NR-AI-ML-PositioningRequestCapabilities*

The IE *NR-AI-ML-PositioningRequestCapabilities* is used by the location server to request the capability of the target device to support NR AI/ML direct positioning and to request NR AI/ML positioning capabilities from a target device.

-- ASN1START

NR-AI-ML-PositioningRequestCapabilities-r19 ::= SEQUENCE {

...

}

-- ASN1STOP

#### 6.5.13.8 NR AI/ML Positioning Error Elements

#### – *NR-AI-ML-Positioning-Error*

The IE *NR-AI-ML-Positioning-Error* is used by the location server or target device to provide NR AI/ML positioning error reasons to the target device or location server, respectively.

-- ASN1START

NR-AI-ML-Positioning-Error-r19 ::= CHOICE {

locationServerErrorCauses-r19 NR-DL-AI-ML-LocationServerErrorCauses-r19,

targetDeviceErrorCauses-r19 NR-DL-AI-ML-TargetDeviceErrorCauses-r19,

...

}

-- ASN1STOP

#### – *NR-DL-AI-ML-LocationServerErrorCauses*

The IE *NR-DL-AI-ML-LocationServerErrorCauses* is used by the location server to provide NR AI/ML positioning error reasons to the target device.

-- ASN1START

NR-DL-AI-ML-LocationServerErrorCauses-r19 ::= SEQUENCE {

cause-r19 ENUMERATED { undefined,

assistanceDataNotSupportedByServer,

assistanceDataSupportedButCurrentlyNotAvailableByServer,

notProvidedAssistanceDataNotSupportedByServer,

on-demand-dl-prs-NotSupportedByServer,

on-demand-dl-prs-SupportedButCurrentlyNotAvailableByServer,

...

},

...

}

-- ASN1STOP

Editor's Note: The above list of error causes is FFS.

#### – *NR-DL-AI-ML-TargetDeviceErrorCauses*

The IE *NR-DL-AI-ML-TargetDeviceErrorCauses* is used by the target device to provide NR AI/ML positioning error reasons to the location server.

-- ASN1START

NR-DL-AI-ML-TargetDeviceErrorCauses-r19 ::= SEQUENCE {

cause-r19 ENUMERATED { undefined,

assistance-data-missing,

unableToMeasureAnyTRP,

attemptedButUnableToMeasureSomeNeighbourTRPs,

thereWereNotEnoughSignalsReceived,

locationCalculationAssistanceDataMissing,

...

},

remoteUE-Indication-r18 ENUMERATED {true} OPTIONAL, -- Cond NR

...

}

-- ASN1STOP

Editor's Note: The above list of error causes is FFS.

| Conditional presence | Explanation |
| --- | --- |
| *NR* | This field is optionally present, need OR, for NR access. Otherwise it is not present. |

| *NR-DL-AI-ML-TargetDeviceErrorCauses* field descriptions |
| --- |
| ***remoteUE-Indication***  This field indicates whether the target device in NR access is configured as a L2 U2N Remote UE. |

## 6.6 Multiplicity and type constraint values

#### *– Multiplicity and type constraint definitions*

-- ASN1START

maxEARFCN INTEGER ::= 65535 -- Maximum value of EUTRA carrier frequency

maxEARFCN-Plus1 INTEGER ::= 65536 -- Lowest value extended EARFCN range

maxEARFCN2 INTEGER ::= 262143 -- Highest value extended EARFCN range

maxMBS-r14 INTEGER ::= 64

maxWLAN-AP-r13 INTEGER ::= 64

maxKnownAPs-r14 INTEGER ::= 2048

maxVisibleAPs-r14 INTEGER ::= 32

maxWLAN-AP-r14 INTEGER ::= 128

maxWLAN-DataSets-r14 INTEGER ::= 8

maxBT-Beacon-r13 INTEGER ::= 32

maxBT-BeaconAntElt-r18 INTEGER ::= 74

maxBT-BeaconAD-r18 INTEGER ::= 64

nrMaxBands-r16 INTEGER ::= 1024 -- Maximum number of supported bands in

-- UE capability.

nrMaxFreqLayers-r16 INTEGER ::= 4 -- Max freq layers

nrMaxFreqLayers-1-r16 INTEGER ::= 3

nrMaxNumDL-PRS-ResourcesPerSet-1-r16 INTEGER ::= 63

nrMaxNumDL-PRS-ResourceSetsPerTRP-1-r16 INTEGER ::= 7

nrMaxResourceIDs-r16 INTEGER ::= 64 -- Max Resource IDs

nrMaxResourceOffsetValue-1-r16 INTEGER ::= 511

nrMaxResourcesPerSet-r16 INTEGER ::= 64 -- Maximum resources for one set

nrMaxSetsPerTrpPerFreqLayer-r16 INTEGER ::= 2 -- Maximum resource sets for one TRP

nrMaxSetsPerTrpPerFreqLayer-1-r16 INTEGER ::= 1

nrMaxTRPs-r16 INTEGER ::= 256 -- Max TRPs per UE

nrMaxTRPsPerFreq-r16 INTEGER ::= 64 -- Max TRPs per freq layers

nrMaxTRPsPerFreq-1-r16 INTEGER ::= 63

maxSimultaneousBands-r16 INTEGER ::= 4 -- Maximum number of simultaneously

-- measured bands

maxBandComb-r16 INTEGER ::= 1024

nrMaxConfiguredBands-r16 INTEGER ::= 16

maxNumOfRxTEGs-r17 INTEGER ::= 32

maxNumOfRxTEGs-1-r17 INTEGER ::= 31

maxNumOfTxTEGs-1-r17 INTEGER ::= 7

maxTxTEG-Sets-r17 INTEGER ::= 256 -- Maximum applicable number is 64

maxNumOfRxTxTEGs-1-r17 INTEGER ::= 255

maxNumOfTRP-TxTEGs-1-r17 INTEGER ::= 7

maxNumOfSRS-PosResources-r17 INTEGER ::= 64

maxNumOfSRS-PosResources-1-r17 INTEGER ::= 63

maxNumResourcesPerAngle-r17 INTEGER ::= 24

maxNumPrioResources-r17 INTEGER ::= 24

maxAddMeasTDOA-r17 INTEGER ::= 31

maxAddMeasAoD-r17 INTEGER ::= 23

maxAddMeasRTT-r17 INTEGER ::= 31

maxOD-DL-PRS-Configs-r17 INTEGER ::= 8

maxCellIDsPerArea-r17 INTEGER ::= 256

maxNrOfAreas-r17 INTEGER ::= 16

maxMeasInstances-r17 INTEGER ::= 32

nrMaxNumPRS-BandWidthAggregation-r18 INTEGER ::= 256 -- Max number of DL-PRS bandwidth

-- aggregation configurations that a

-- location server can provide to a UE

nrNumOfSamples-r18 INTEGER ::= 4 -- NSample of RSCP/RSCPD

nrNumOfSamples-1-r18 INTEGER ::= 3

-- ASN1STOP

#### *– End of LPP-PDU-Definitions*

-- ASN1START

END

-- ASN1STOP

# 7 Broadcast of assistance data

## 7.1 General

Broadcast of positioning assistance data is supported via Positioning System Information Blocks (posSIBs) as specified in TS 36.331 [12] or TS 38.331 [35]. The posSIBs are carried in RRC System Information (SI) messages (TS 36.331 [12] or TS 38.331 [35]).

For LTE RRC System Information (SI), a single *SystemInformationBlockPos* IE is defined in TS 36.331 [12] which is carried in IE *PosSystemInformation-r15-IEs* specified in TS 36.331 [12]. The mapping of positioning SIB type (*posSibType*) to assistance data carried in *SystemInformationBlockPos* is specified in clause 7.2.

For NR RRC System Information (SI), a single *SIBpos* IE is defined in TS 38.331 [35] which is carried in IE *PosSystemInformation-r16-IEs* specified in TS 38.331 [35]. The mapping of positioning SIB type (*posSibType*) to assistance data carried in *SIBpos* is specified in clause 7.2.

## 7.2 Mapping of *posSibType* to assistance data element

The supported *posSibType*'s are specified in Table 7.2-1. The GNSS Common and Generic Assistance Data IEs are defined in clause 6.5.2.2. The OTDOA Assistance Data IEs and NR DL-TDOA/DL-AoD Assistance Data IEs are defined in clause 7.4.2. The Barometric Assistance Data IEs are defined in clause 6.5.5.8. The TBS (based on MBS signals) Assistance Data IEs are defined in clause 6.5.4.8.

Table 7.2-1: Mapping of posSibType to assistanceDataElement

|  |  |  |
| --- | --- | --- |
|  | *posSibType* | *assistanceDataElement* |
| GNSS Common Assistance Data (clause 6.5.2.2) | *posSibType1-1* | *GNSS-ReferenceTime* |
| *posSibType1-2* | *GNSS-ReferenceLocation* |
| *posSibType1-3* | *GNSS-IonosphericModel* |
| *posSibType1-4* | *GNSS-EarthOrientationParameters* |
| *posSibType1-5* | *GNSS-RTK-ReferenceStationInfo* |
| *posSibType1-6* | *GNSS-RTK-CommonObservationInfo* |
| *posSibType1-7* | *GNSS-RTK-AuxiliaryStationData* |
| *posSibType1-8* | *GNSS-SSR-CorrectionPoints* |
| *posSibType1-9* | *GNSS-Integrity-ServiceParameters* |
| *posSibType1-10* | *GNSS-Integrity-ServiceAlert* |
| *posSibType1-11* | *GNSS-LOS-NLOS-GridPoints* |
| *posSibType1-12* | *GNSS-SSR-IOD-Update* |
| GNSS Generic Assistance Data (clause 6.5.2.2) | *posSibType2-1* | *GNSS-TimeModelList* |
| *posSibType2-2* | *GNSS-DifferentialCorrections* |
| *posSibType2-3* | *GNSS-NavigationModel* |
| *posSibType2-4* | *GNSS-RealTimeIntegrity* |
| *posSibType2-5* | *GNSS-DataBitAssistance* |
| *posSibType2-6* | *GNSS-AcquisitionAssistance* |
| *posSibType2-7* | *GNSS-Almanac* |
| *posSibType2-8* | *GNSS-UTC-Model* |
| *posSibType2-9* | *GNSS-AuxiliaryInformation* |
| *posSibType2-10* | *BDS-DifferentialCorrections* |
| *posSibType2-11* | *BDS-GridModelParameter* |
| *posSibType2-12* | *GNSS-RTK-Observations* |
| *posSibType2-13* | *GLO-RTK-BiasInformation* |
| *posSibType2-14* | *GNSS-RTK-MAC-CorrectionDifferences* |
| *posSibType2-15* | *GNSS-RTK-Residuals* |
| *posSibType2-16* | *GNSS-RTK-FKP-Gradients* |
| *posSibType2-17* | *GNSS-SSR-OrbitCorrections* |
| *posSibType2-17a* | *GNSS-SSR-OrbitCorrectionsSet2* |
| *posSibType2-18* | *GNSS-SSR-ClockCorrections* |
| *posSibType2-18a* | *GNSS-SSR-ClockCorrectionsSet2* |
| *posSibType2-19* | *GNSS-SSR-CodeBias* |
| *posSibType2-20* | *GNSS-SSR-URA* |
| *posSibType2-20a* | *GNSS-SSR-URA-Set2* |
| *posSibType2-21* | *GNSS-SSR-PhaseBias* |
| *posSibType2-22* | *GNSS-SSR-STEC-Correction* |
| *posSibType2-23* | *GNSS-SSR-GriddedCorrection* |
| *posSibType2-24* | *NavIC-DifferentialCorrections* |
| *posSibType2-25* | *NavIC-GridModelParameter* |
| *posSibType2-26* | *GNSS-LOS-NLOS-GriddedIndications* |
| *posSibType2-27* | *GNSS-SSR-SatellitePCVResiduals* |
| OTDOA Assistance Data (clause 7.4.2) | *posSibType3-1* | *OTDOA-UE-Assisted* |
| Barometric Assistance Data  (clause 6.5.5.8) | *posSibType4-1* | *Sensor-AssistanceDataList* |
| TBS Assistance Data  (clause 6.5.4.8) | *posSibType5-1* | *TBS-AssistanceDataList* |
| NR DL-TDOA/DL-AoD Assistance Data (clauses 6.4.3, 7.4.2) | *posSibType6-1* | *NR-DL-PRS-AssistanceData* |
| *posSibType6-2* | *NR-UEB-TRP-LocationData* |
| *posSibType6-3* | *NR-UEB-TRP-RTD-Info* |
| *posSibType6-4* | *NR-TRP-BeamAntennaInfo* |
| *posSibType6-5* | *NR-DL-PRS-TRP-TEG-Info* |
| *posSibType6-7* | *NR-PRU-DL-Info* |
| On-demand DL-PRS Configurations (clause 6.4.3) | *posSibType6-6* | *NR-On-Demand-DL-PRS-Configurations* |
| Integrity Assistance Data for NR Positioning Methods (clause 6.4.3) | *posSibType7-1* | *NR-IntegrityRiskParameters* |
| *posSibType7-2* | *NR-IntegrityServiceParameters* |
| *posSibType7-3* | *NR-IntegrityServiceAlert* |
| *posSibType7-4* | *NR-IntegrityParameters* |

## 7.3 Procedures related to broadcast information elements

Upon receiving *AssistanceDataSIBelement*, the target device shall:

1> if the *segmentationInfo* is not included:

2> if the *cipheringKeyData* is included:

3> if the UE has obtained a valid cipher key value and the first portion of the initial Counter denoted C0 corresponding to the *cipherSetID* using NAS signalling:

4> if C0 contains less than 128-bits:

5> pad out the bit string with zeroes in most significant bit positions to achieve 128 bits.

4> if the *d0* field contains less than 128-bits:

5> pad out the bit string with zeroes in least significant bit positions to achieve 128 bits, denoted D0.

4> determine the initial Counter C1 = (C0 + D0) mod 2128 (where all values are treated as non-negative integers);

4> determine any subsequent counter Ci from the previous counter Ci-1 as Ci = (Ci-1 + 1) mod 2128;

4> use the sequence of counters <C1, C2, C3, …> and the cipher key value to decipher the *assistanceDataElement;*

4> decode the deciphered *assistanceDataElement* and deliver the related assistance data to upper layers.

3> else:

4> discard the *AssistanceDataSIBelement.*

2> else:

3> decode the *assistanceDataElement* and deliver the related assistance data to upper layers.

1> else:

2> if *segmentationOption* indicates '*pseudo-seg*':

3> if the *cipheringKeyData* is included:

4> if the UE has obtained a valid cipher key value and the first portion of the initial Counter denoted C0 corresponding to the *cipherSetID* using NAS signalling:

5> if C0 contains less than 128-bits:

6> pad out the bit string with zeroes in most significant bit positions to achieve 128 bits.

5> if the *d0* field contains less than 128-bits:

6> pad out the bit string with zeroes in least significant bit positions to achieve 128 bits, denoted D0.

5> determine the initial Counter C1 = (C0 + D0) mod 2128 (where all values are treated as non-negative integers);

5> determine any subsequent counter Ci from the previous counter Ci-1 as Ci = (Ci-1 + 1) mod 2128;

5> use the sequence of counters <C1, C2, C3, …> and the cipher key value to decipher the *assistanceDataElement* segment*;*

5> decode the deciphered *assistanceDataElement* segment and deliver the related assistance data portion together with the *assistanceDataSegmentType* and *assistanceDataSegmentNumber* to upper layers.

4> else:

5> discard the *AssistanceDataSIBelement* segment.

3> else:

4> decode the *assistanceDataElement* segment and deliver the related assistance data portion together with the *assistanceDataSegmentType* and *assistanceDataSegmentNumber* to upper layers.

2> if *segmentationOption* indicates '*octet-string-seg*':

3> if all segments of *assistanceDataElement* have been received:

4> assemble the assistance data element from the received *assistanceDataElement* segments;

5> if the *cipheringKeyData* is included in the first segment:

6> if the UE has obtained a valid cipher key value and the first portion of the initial Counter denoted C0 corresponding to the *cipherSetID* using NAS signalling:

7> if C0 contains less than 128-bits:

8> pad out the bit string with zeroes in most significant bit positions to achieve 128 bits.

7> if the *d0* field contains less than 128-bits:

8> pad out the bit string with zeroes in least significant bit positions to achieve 128 bits, denoted D0.

7> determine the initial Counter C1 = (C0 + D0) mod 2128 (where all values are treated as non-negative integers);

7> determine any subsequent counter Ci from the previous counter Ci-1 as Ci = (Ci-1 + 1) mod 2128;

7> use the sequence of counters <C1, C2, C3, …> and the cipher key value to decipher the assembled assistance data element;

7> decode the assembled and deciphered assistance data element and deliver the related assistance data to upper layers.

6> else:

7> discard the assembled assistance data element.

5> else:

6> decode the assembled assistance data element and deliver the related assistance data to upper layers.

NOTE: As an optional optimisation when *segmentationOption* indicates '*octet-string-seg*', a target device may verify if the *cipheringKeyData* is included in the first segment as soon as the first segment is received and, if included, may verify that the UE has obtained a valid cipher key value and the first portion of the initial Counter denoted C0 corresponding to the *cipherSetID* using NAS signalling. When the UE has not obtained a valid cipher key value and initial Counter C0 using NAS signalling, the UE may discard the first segment and ignore all subsequent segments.

The value for D0 shall be different for different *AssistanceDataSIBelement*'s to ensure that the counters derived from C1 for any *assistanceDataElement* are different to the counters for any other *assistanceDataElement* for a given ciphering key.

D0 shall contain at least 16 least significant bits (LSBs) set to zero to ensure that the values of D0 differ from another by a large value.

## 7.4 Broadcast information elements

### 7.4.1 Basic production

This clause defines the LPP broadcast information elements which are encoded as 'basic production' for system information broadcast purposes (see TS 36.331 [12], TS 38.331 [35]).

The 'basic production' is obtained from their ASN.1 definitions by use of Basic Packed Encoding Rules (BASIC-PER), Unaligned Variant, as specified in ITU-T Rec. X.691 [22]. It always contains a multiple of 8 bits.

#### *– LPP-Broadcast-Definitions*

This ASN.1 segment is the start of the LPP Broadcast definitions.

-- ASN1START

LPP-Broadcast-Definitions

DEFINITIONS AUTOMATIC TAGS ::=

BEGIN

IMPORTS

OTDOA-ReferenceCellInfo,

OTDOA-NeighbourCellInfoList,

NR-TRP-LocationInfo-r16,

NR-DL-PRS-BeamInfo-r16,

NR-RTD-Info-r16,

NR-IntegrityParametersTRP-LocationInfo-r18,

NR-IntegrityParametersDL-PRS-BeamInfo-r18,

NR-IntegrityParametersRTD-Info-r18,

NR-IntegrityParametersTRP-BeamAntennaInfo-r18

FROM LPP-PDU-Definitions;

-- ASN1STOP

### 7.4.2 Element definitions

#### – *AssistanceDataSIBelement*

The IE *AssistanceDataSIBelement* is used in the IE *SystemInformationBlockPos* as specified in TS 36.331 [12] andIE *SIBpos* as specified in TS 38.331 [35].

-- ASN1START

AssistanceDataSIBelement-r15 ::= SEQUENCE {

valueTag-r15 INTEGER (0..63) OPTIONAL, -- Need OP

expirationTime-r15 UTCTime OPTIONAL, -- Need OP

cipheringKeyData-r15 CipheringKeyData-r15 OPTIONAL, -- Need OP

segmentationInfo-r15 SegmentationInfo-r15 OPTIONAL, -- Need OP

assistanceDataElement-r15 OCTET STRING,

...

}

CipheringKeyData-r15 ::= SEQUENCE {

cipherSetID-r15 INTEGER (0..65535),

d0-r15 BIT STRING (SIZE (1..128)),

...

}

SegmentationInfo-r15 ::= SEQUENCE {

segmentationOption-r15 ENUMERATED {pseudo-seg, octet-string-seg},

assistanceDataSegmentType-r15 ENUMERATED {notLastSegment, lastSegment},

assistanceDataSegmentNumber-r15 INTEGER (0..63),

...

}

-- ASN1STOP

| *AssistanceDataSIBelement* field descriptions |
| --- |
| ***valueTag***  This field is used to indicate to the target device any changes in the broadcast assistance data content. The *valueTag* is incremented by one, by the location server, every time a modified assistance data content is provided. This field is not included if the broadcast assistance data changes too frequently. If *valueTag* and *expirationTime* are absent, the UE assumes that the broadcast assistance data content changes at every broadcast interval. |
| ***expirationTime***  This field indicates how long the broadcast assistance data content is valid. It is specified as UTC time and indicates when the broadcast assistance data content will expire. |
| ***cipheringKeyData***  If present, indicates that the *assistanceDataElement* octet string is ciphered. |
| ***segmentationInfo***  If present, indicates that the *assistanceDataElement* is one of many segments. |
| ***assistanceDataElement***  The *assistanceDataElement* OCTET STRING depends on the *posSibType* and is specified in Table 7.2-1. NOTE. |
| ***cipherSetID***  This field identifies a cipher set comprising a cipher key value and the first component C0 of the initial counter C1. |
| ***d0***  This field provides the second component for the initial ciphering counter C1. This field is defined as a bit string with a length of 1 to 128 bits. A target device first pads out the bit string if less than 128 bits with zeroes in least significant bit positions to achieve 128 bits. C1 is then obtained from D0 and C0 (defined by the *cipherSetID*) as:  C1 = (D0 + C0) mod 2128 (with all values treated as non-negative integers). |
| ***segmentationOption***  Indicates the used segmentation option. |
| ***assistanceDataSegmentType***  Indicates whether the included *assistanceDataElement* segment is the last segment or not. |
| ***assistanceDataSegmentNumber***  Segment number of the *assistanceDataElement* segment. A segment number of zero corresponds to the first segment, one corresponds to the second segment, and so on. Segments numbers wraparound should there be more than 64 segments |

NOTE: For example, if the *posSibType* in IE *PosSIB-Type* defined in TS 36.331 [12] and TS 38.331 [35] indicates '*posSibType1-7*', the *assistanceDataElement* OCTET STRING includes the LPP IE *GNSS‑RTK‑AuxiliaryStationData*.

#### – *OTDOA-UE-Assisted*

The IE *OTDOA-UE-Assisted* is used in the *assistanceDataElement* if the *posSibType* in IE *PosSIB-Type* defined in TS 36.331 [12] indicates '*posSibType3-1*'.

-- ASN1START

OTDOA-UE-Assisted-r15 ::= SEQUENCE {

otdoa-ReferenceCellInfo-r15 OTDOA-ReferenceCellInfo,

otdoa-NeighbourCellInfo-r15 OTDOA-NeighbourCellInfoList,

...

}

-- ASN1STOP

| *OTDOA-UE-Assisted* field descriptions |
| --- |
| ***otdoa-ReferenceCellInfo***  LPP IE *OTDOA-ReferenceCellInfo* as defined in clause 6.5.1.2. |
| ***otdoa-NeighbourCellInfo***  LPP IE *OTDOA-NeighbourCellInfoList* as defined in clause 6.5.1.2. |

#### – *NR-UEB-TRP-LocationData*

The IE *NR-UEB-TRP-LocationData* is used in the *assistanceDataElement* if the *posSibType* in IE *PosSIB-Type* defined in TS 38.331 [35] indicates '*posSibType6-2*'.

-- ASN1START

NR-UEB-TRP-LocationData-r16 ::= SEQUENCE {

nr-trp-LocationInfo-r16 NR-TRP-LocationInfo-r16,

nr-dl-prs-BeamInfo-r16 NR-DL-PRS-BeamInfo-r16 OPTIONAL, -- Need ON

...

}

-- ASN1STOP

| *NR-UEB-TRP-LocationData* field descriptions |
| --- |
| ***nr-trp-LocationInfo***  LPP IE *NR-TRP-LocationInfo* as defined in clause 6.4.2.1. |
| ***nr-dl-prs-BeamInfo***  LPP IE *NR-DL-PRS-Beam-Info* as defined in clause 6.4.2.1. |

#### – *NR-UEB-TRP-RTD-Info*

The IE *NR-UEB-TRP-RTD-Info* is used in the *assistanceDataElement* if the *posSibType* in IE *PosSIB-Type* defined in TS 38.331 [35] indicates '*posSibType6-3*'.

-- ASN1START

NR-UEB-TRP-RTD-Info-r16 ::= SEQUENCE {

nr-rtd-Info-r16 NR-RTD-Info-r16,

...

}

-- ASN1STOP

| *NR-UEB-TRP-RTD-Info* field descriptions |
| --- |
| ***nr-rtd-Info***  LPP IE *NR-RTD-Info* as defined in clause 6.4.2.1. |

#### – *NR-IntegrityParameters*

The IE *NR-IntegrityParameters* is used in the *assistanceDataElement* if the *posSibType* in IE *SIB-TypeInfo-v1700* defined in TS 38.331 [35] indicates '*posSibType7-4*'.

-- ASN1START

NR-IntegrityParameters-r18 ::= SEQUENCE {

nr-IntegrityParametersTRP-LocationInfo-r18

NR-IntegrityParametersTRP-LocationInfo-r18 OPTIONAL, -- Need OR

nr-IntegrityParametersDL-PRS-BeamInfo-r18

NR-IntegrityParametersDL-PRS-BeamInfo-r18 OPTIONAL, -- Need OR

nr-IntegrityParametersRTD-Info-r18

NR-IntegrityParametersRTD-Info-r18 OPTIONAL, -- Need OR

nr-IntegrityParametersTRP-BeamAntennaInfo-r18

NR-IntegrityParametersTRP-BeamAntennaInfo-r18 OPTIONAL, -- Need OR

...

}

-- ASN1STOP

| *NR-IntegrityParameters* field descriptions |
| --- |
| ***nr-IntegrityParametersTRP-LocationInfo***  LPP IE *NR-IntegrityParametersTRP-LocationInfo* as defined in IE *NR-PositionCalculationAssistance* in clause 6.4.3. |
| ***nr-IntegrityParametersDL-PRS-BeamInfo***  LPP IE *NR-IntegrityParametersDL-PRS-BeamInfo* as defined in IE *NR-PositionCalculationAssistance* in clause 6.4.3. |
| ***nr-IntegrityParametersRTD-Info***  LPP IE *NR-IntegrityParametersRTD-Info* as defined in IE *NR-PositionCalculationAssistance* in clause 6.4.3. |
| ***nr-IntegrityParametersTRP-BeamAntennaInfo***  LPP IE *NR-IntegrityParametersTRP-BeamAntennaInfo* as defined in IE *NR-PositionCalculationAssistance* in clause 6.4.3. |

#### *– End of LPP-Broadcast-Definitions*

-- ASN1START

END

-- ASN1STOP

## 7.5 Broadcast ciphering (informative)

The *assistanceDataElement* OCTET STRING included in IE *AssistanceDataSIBelement* may be ciphered using the 128-bit Advanced Encryption Standard (AES) algorithm (with counter mode).

AES as specified in [32] and [33] is a block mode cipher algorithm that ciphers blocks of 128 bits at a time. However, Counter mode enables usage for a bit string that is not an exact multiple of 128 bits. Further, Counter mode enables a target (or a server) to perform most of the deciphering (or ciphering) processing independently of receipt of the data to be deciphered (or ciphered) which may enable more efficient processing. Provided counters are chosen in a non‑repeating manner by the server (which is a requirement for Counter mode), every block of data will be ciphered in a unique manner.

The algorithm makes use of a sequence of counters <C1, C2, C3, …> each containing 128 bits, where C1 is specified by the server and each subsequent counter (C2, C3 etc.) is obtained from the previous counter by adding one modulo 2128. Each counter Ci is ciphered using the AES algorithm with a common 128-bit key to produce an output block Oi of 128 bits. To perform ciphering, the *assistanceDataElement* is divided into blocks B1, B2, … Bn of 128 bits each, except for the last block Bn which may contain fewer than 128 bits. The ciphered *assistanceDataElement* is obtained as a sequence of *n* blocks containing 128 bits each (except possibly for the last block) given by (O1 XOR B1), (O2 XOR B2), … (On XOR Bn), where XOR denotes bitwise exclusive OR. In the case of the last block, if Bn contains *m* bits (*m*<128), then the *m* most significant bits of On would be used for the exclusive OR. Deciphering is performed in the same way except that the blocks B1, B2, … Bn are now obtained from the ciphered message and the result of the exclusive OR operations yields the original unciphered message. Figure 7.5-1 provides an illustration of Counter mode for the generic case of an arbitrary block cipher algorithm CIPHk.



Figure 7.5-1: Illustration of Block Ciphering with Counter Mode [33].

The algorithms require specific conventions for bit ordering. The bit ordering applicable to ciphering for a ASN.1 PER encoded *assistanceDataElement* is the bit ordering produced by the ASN.1 PER encoding where the first bit is the leading bit number zero, the second bit is bit one etc..

The initial counter C1 used to cipher an entire *assistanceDataElement* is provided to a target by a server in two portions. The first portion, denoted C0, is provided using point to point mode along with the 128-bit ciphering key and an identifier for both of these values as specified in TS 23.271 [3]. The second portion, denoted D0 (*d0*), is provided in unciphered form in IE *CipheringKeyData*. A target then obtains C1 as:

C1 = (C0 + D0) mod 2128 (where all values are treated as non-negative integers)

To obtain any subsequent counter Ci from the previous counter Ci1 for any message, the following operation is used:

Ci = (Ci1 + 1) mod 2128

NOTE: As specified in clause 7.3 the value for D0 is different for different *AssistanceDataSIBelement*'s to ensure that the counters derived from C1 for any *assistanceDataElement* can be different to the counters for any other *assistanceDataElement*. However, a long *assistanceDataElement* or a segmented *assistanceDataElement* would require the use of consecutive counter values C1 to Cn, where *n* is the *assistanceDataElement* size in bits divided by 128 (and rounded up). There would then be a danger of small changes in the value of D0 for ciphering of different *assistanceDataElement*'s (e.g. D0 being chosen as 1 larger than a previous D0 value) reusing previous counter values. To avoid this, the values of D0 contain 16 least significant bits (LSBs) set to zero, as specified in clause 7.3.

# Annex A:

# RAN2 Agreements

## RAN2#125bis

General:

* RAN2 confirms that UE will not be informed about any gNB/LMF-sided model/functionality management decision (e.g., selection, (de)activation, switching, fallback, etc.)
* RAN2 confirms that UE will not be involved in any gNB/LMF-sided model/functionality management decision making (e.g., selection, (de)activation, switching, fallback, etc.), except being configured to provide the required measurement/data.
* RAN2 focuses on the data collection procedure from UE to NW (e.g., gNB, LMF, or OAM) for the sake of NW-sided model LCM (including training, inference, management).
* Support proactive reporting of UE-sided applicable functionality, e.g., the UE reports its applicable AI/ML functionalities via UAI message/LPP message
* Support reactive reporting of UE-sided applicable functionality. The NW configures AI/ML functionalities via RRC/LPP message. FFS what the configuration contains. FFS how to report applicable functionality and what is applicable functionality

Pos:

* For POS, RAN2 assumes gNB or LMF could perform performance monitoring for case 3a and LMF is responsible for the performance monitoring for case 3b and wait for any further inputs from other WGs.
* For POS, RAN2 assumes that NRPPa is used for the signalling between gNB and LMF for case 3a and 3b and the detailed signalling design is up to RAN3.

## RAN2#126

General:

* The UE will indicate the gNB/LMF whether the AI/ML functionality is available/applicable. For a functionality to be applicable at least there should at least one model available within it. FFS other details on what is applicability/non-applicability.

Pos:

* RAN2 to await RAN1 progress to determine need for any specification work on AI/ML positioning Case 3a and Case 3b.
* The LPP Capability Transfer procedures (RequestCapabilities/ProvideCapabilities messages) are used to indicate supported AI/ML positioning capabilities. FFS how to handle dynamic capabilities, depending on further RAN1 progress and understanding of the functionality.
* Wait for RAN1 for associate ID discussion
* At least for Case 1, existing LPP procedures related to Location Information Transfer (RequestLocationInformation/ ProvideLocationInformation messages) are used for providing the results of the UE sided model inference operation. FFS further details on signaling enhancements

## RAN2#127

General:

* Supported functionalities refer to functionalities that UE can indicate by using UE capability information (via RRC/LPP signalling)

## RAN2#127bis

* The following procedures for LCM for UE sided model for AI positioning case 1 is the baseline:
  + Step 1: LMF may request the UE to report the supported functionalities at the UE side by LPP request capabilities message.
  + Step 2: UE sends LPP provide capabilities message to LMF with the supported functionalities at the UE side.
  + Step 3: LMF sends the LPP provide assistance data message (which may contain network side additional condition).
  + Step 4: UE reports the applicable functionality to the LMF by the LPP provide capabilities message.
  + Step 5: The LMF requests the inferred location information using the LPP request location information message.
  + Step 6: UE reports the inferred location using LPP provide location information message.
* Whether the inference configuration is provided in step 3 or/and step 5 is FFS (to be revised based on RAN1 progress).
* Whether network side additional condition is needed and what it contains is FFS (to be revised based on RAN1 progress).
* FFS whether LMF controls the UE sending unsolicited LPP provide capabilities (i.e. whether step4 is sent reactively or proactively). FFS the signalling details.
* RAN2 will decide whether AI positioning will be a new method after further details from RAN1 are received.

## RAN2#128

* For POS Case 1, RAN2 confirm that the existing unsolicited UE capability report mechanism in LPP can support UE to report the applicable functionality in both “proactive” and “reactive” as a baseline.
  + Proactive case: When the applicability change, UE can send an unsolicited LPP ProvideCapabilities message to LMF.
  + Reactive case: If the applicability changes based on the configuration in LPP ProvideAssistanceData message in step 3, UE can send an unsolicited LPP ProvideCapabilities message to LMF. Configuration details are FFS.
* As a baseline, If the AIML based positioning method becomes non-applicable when LMF requests UE location estimation, UE cannot perform the AIML based positioning, and reply with LPP Providelocationinformation message with error cause. FFS if other fallback options are considered.

## RAN2#129

* RAN2 has not and will not study Case 2a and Case 2b in Rel-19. An LS was sent to SA2 to notify this agreement (LS available in R2-2501507)
* Introduce AI/ML positioning Case 1 as a new positioning method
* Existing LPP procedures related to Location Information Transfer (RequestLocationInformation/ ProvideLocationInformation messages) are used for providing and requesting the results of the UE sided model inference operation. The detail stage 3 message extention can be disucssed while drafting the stage 3 CR.
* FFS UE autonomous switching between AI/ML and non-AI/ML methods is not allowed. FFS if this is unconditional or linked to condition of multiple positioning method are not configured in RequestLocationInformation.
* The content of error cause is discussed while drafting stage3 CRs.
* As a baseline, UE receives the needed assistance data for calculating UE location for AI/ML in step3 (ProvideAssistanceData) and UE receives the instruction to perform the inference in step 5 (RequestLocationInformation). The content of Assistance Data and the content of request location information is based upon RAN1 parameter list.
* UE reports the applicable functionality to the LMF by the LPP provide capabilities message if there is a change of applicable functionality. FFS if any additional LMF control is needed.

## RAN2#129bis

* LMF is responsible for functionality management
* UE reports the applicable functionality to the LMF by the LPP provide capabilities message without any additional LMF control.
* Switching/fallback to non-AI/ML positioning can be supported by including multiple positioning methods in a LPP Request Location Information message. No additional specification work is foreseen specifically for supporting "switching/fallback operation".
* An AIML positioning functionality is considered “activated” once UE receives an LPP RequestLocationInformation from the LMF requesting inferred location information.
* For triggered and periodical reporting, we rely on existing positioning framework mechanisms to deactivate AI/ML positioning (no spec impact is foreseen)

# RAN1 Agreements related to Case 1

## RAN1#116bis

**Working Assumption**

For training data generation of AI/ML based positioning Case 1, the measurement and its related data (e.g., timestamp) are generated by PRU and/or Non-PRU UE.

**Working Assumption**

For training data generation of AI/ML based positioning Case 1, the label and its related data (e.g., time stamp) can be generated by:

* PRU
* Non-PRU UE with estimated location
* LMF

Note: transfer of the label and its related data is out of RAN1 scope.

**Agreement**

For model performance monitoring of AI/ML positioning Case 1, for model performance monitoring metric calculation in label-based model monitoring, study the feasibility, benefits, and potential specification impact of the following options with regard to how to generate information on ground truth label:

* Option A. The target UE side performs monitoring metric calculation.
  + Option A-1. At least information on ground truth label of the target UE is generated by LMF and provided to the target UE.
    - In one example, target UE and/or gNB sends measurement (e.g., legacy measurement) to LMF so that LMF can derive the information on ground truth label.
  + Option A-2. At least position calculation assistance data (e.g., existing information for UE-based positioning method) is provided from LMF to the target UE.
  + Option A-3. Reuse Rel-18 assistance data transfer framework from LMF to the target UE, where the PRU measurement (e.g., legacy measurement) and the corresponding PRU location are sent via LMF to the target UE.
  + Option A-4. PRU measurement (and the corresponding PRU location if not already known at the UE-side) are sent from PRU to the target UE side ~~(e.g., target UE, OTT server)~~.
    - Note: Option A-4 can be realized by implementation in a manner transparent to specification if the PRU sends information to the target UE side in a proprietary method.
* Option B. The LMF performs monitoring metric calculation.
  + Option B-1. at least inference result (i.e., the model output corresponding to target UE’s channel measurement) of the target UE is sent by the target UE to LMF.
  + Option B-2. PRU’s channel measurement is sent via LMF to the target UE, and the inference result (i.e., the model output corresponding to PRU’s channel measurement) is sent by the target UE to LMF.

Note: exact method to perform the monitoring metric calculation is up to implementation.

Note: Other options are not precluded.

## RAN1#118

**Conclusion**

For model performance monitoring of AI/ML positioning Case 1, for model performance monitoring metric calculation in label-based model monitoring,

* Option A-4 can be realized by implementation in a manner transparent to specification specification if the PRU sends information to the target UE side in a proprietary method. No further discussion on Option A-4.

**Agreement**

For training data collection of Case 1 and 2a, in terms of DL PRS configuration for collecting training data, RAN1 study the following options on assistance data, using legacy mechanisms as a starting point:

Option A. (UE initiated) UE makes a request to LMF on the preferred DL PRS configuration for training data collection, e.g., on-demand PRS. LMF makes the decision on determining the DL PRS configuration for training data collection and provides the assistance data to the UE.

Option B. (LMF initiated) LMF determines the DL PRS configuration for training data collection and provides the assistance data to the UE.

Note: the UE can be a PRU and/or a Non-PRU UE.

Note: as in existing specification, the DL PRS configurations in the assistance data from LMF to UE are based on DL PRS configuration coordinated between LMF and gNB.

## RAN1#118bis

**Conclusion**

For training data collection of Case 1, in terms of DL PRS configuration for collecting training data, both options are feasible by using legacy mechanisms:

Option A. (UE initiated) UE makes a request to LMF on the preferred DL PRS configuration for training data collection, e.g., on-demand PRS. LMF makes the decision on determining the DL PRS configuration for training data collection and provides the assistance data to the UE.

Option B. (LMF initiated) LMF determines the DL PRS configuration for training data collection and provides the assistance data to the UE.

Note: the UE can be a PRU and/or a Non-PRU UE.

Note: as in existing specification, the DL PRS configurations in the assistance data from LMF to UE are based on DL PRS configuration coordinated between LMF and gNB.

**Agreement**

For AI/ML positioning Case 1, regarding the assistance data provided from LMF to UE, for ensuring consistency between training and inference,

* for each of the existing assistance data IE of UE-based DL-TDOA and/or UE-based DL-AoD, study whether it should be: (a) explicitly indicated, (b) implicitly indicated and/or (c) other;
* Companies can provide inputs on further enhancements of existing assistance data, including new information
* Note: this does not mean that training and inference phases are mentioned in assistance data.

Table. Existing assistance data (supported up to Rel-18) that may be transferred from LMF to UE in UE-based DL-TDOA [1] or UE-based DL-AoD [2], as applicable.

|  |  |  |  |
| --- | --- | --- | --- |
|  | **Information** | **UE-based DL-TdoA** | **UE-based DL-AoD** |
| 1 | Physical cell IDs (PCIs), global cell IDs (GCIs), ARFCN, and PRS IDs of candidate NR TRPs for measurement |  |  |
| 2 | Timing relative to the serving (reference) TRP of candidate NR TRPs |  |  |
| 3 | DL-PRS configuration of candidate NR TRPs |  |  |
| 4 | Indication of which DL-PRS Resource Sets across DL-PRS positioning frequency layers are linked for DL-PRS bandwidth aggregation |  |  |
| 5 | SSB information of the TRPs (the time/frequency occupancy of SSBs) |  |  |
| 6 | Spatial direction information (e.g. azimuth, elevation etc.) of the DL-PRS Resources of the TRPs served by the gNB |  |  |
| 7 | Geographical coordinates of the TRPs served by the gNB (include a transmission reference location for each DL-PRS Resource ID, reference location for the transmitting antenna of the reference TRP, relative locations for transmitting antennas of other TRPs) |  |  |
| 8 | Fine Timing relative to the serving (reference) TRP of candidate NR TRPs |  |  |
| 9 | PRS-only TP indication |  |  |
| 10 | The association information of DL-PRS resources with TRP Tx TEG ID |  |  |
| 11 | LOS/NLOS indicators |  |  |
| 12 | On-Demand DL-PRS-Configurations, possibly together with information on which configurations are available for DL-PRS bandwidth aggregation |  |  |
| 13 | Validity Area of the Assistance Data |  |  |
| 14 | PRU measurements together with the location information of the PRU |  |  |
| 15 | Data facilitating the integrity results determination of the calculated location |  |  |
| 16 | TRP beam/antenna information (including azimuth angle, zenith angle and relative power between PRS resources per angle per TRP) |  |  |
| 17 | Expected Angle Assistance information |  |  |
| 18 | PRS priority list |  |  |

[1] Table 8.12.2.1.0-1 in 38.305, Use equipment (UE) positioning in NG-RAN (Release 18), v18.3.0

[2] Table 8.11.2.1.0-1 in 38.305, Use equipment (UE) positioning in NG-RAN (Release 18), v18.3.0

## RAN1#119

**Agreement**

For model performance monitoring of AI/ML positioning Case 1, support at least:

* Option A. The target UE side performs monitoring metric calculation.
  + The target UE may signal the monitoring outcome to the LMF.
  + FFS: content of monitoring outcome
* FFS: Option B

**Agreement**

For AI/ML based positioning Case 1, all assistance information from legacy UE-based DL-TDOA, other than info #7, can be provided from LMF to UE. For info #7, RAN1 study, if necessary, choose one alternative from the following:

* Alternative 1. Info #7 is provided implicitly via associated ID.
  + Associated ID is signaled by LMF to indicate whether info #7 is consistent between training and inference.
* Alternative 2. Info #7 can be provided either implicitly or explicitly by LMF. Note: no UE capability is introduced on whether info #7 is provided implicitly or explicitly, and the UE can request info #7 to be provided explicitly or implicitly.
  + If provided implicitly, associated ID is signaled by LMF to indicate whether info #7 is consistent between training and inference.
* Alternative 3. Info #7 is **not** be provided from LMF to UE.
  + If info #7 is not provided, UE may assume info #7 is consistent between training and inference.
* Alternative 4. Info #7 is provided explicitly from LMF to UE.

|  |  |
| --- | --- |
| 7 | Geographical coordinates of the TRPs served by the gNB (include a transmission reference location for each DL-PRS Resource ID, reference location for the transmitting antenna of the reference TRP, relative locations for transmitting antennas of other TRPs) |

## RAN1#120

**Agreement**

For AI/ML based positioning Case 1, from RAN1 perspective, when the label data of location is generated by LMF and transferred from LMF to UE, label and quality indicator of label can be provided by reusing existing IEs.

* From RAN1 perspective, the existing IE can use one of the geographic shapes defined in TS 23.032. The location estimate uncertainty and confidence (if included with the geographic shapes) can serve as quality indicator of the label.

## RAN1#120bis

Agreement

For model performance monitoring of AI/ML positioning Case 1, “FFS: content of monitoring outcome” in RAN1#119 agreement is resolved by:

* the content of monitoring outcome includes at least an indication that the target UE cannot perform the Case 1 positioning method.