**3GPP TSG-RAN WG2 Meeting #130R2-250xxxx**

**St. Julian’s, Malta, 19th - 23th May 2025**

**Agenda item: 8.4.1**

**Source: CATT**

**Title: Collection of comments and open issues on Running CR for 38.304 (CATT)**

**Document for: Discussion and Decision**

# Introduction

This document is the report of the following discussion:

* [Post129bis][208][LPWUS] Running CR for 38.304 (CATT)

Intended outcome: Updated running CR based on new agreements for endorsement, open issue list (if needed)

Deadline: Long (May. 2nd 10:00 UTC)

Companies providing input to this email discussion are requested to leave contact information below.

|  |  |  |
| --- | --- | --- |
| **Company** | **Delegate name** | **Email address** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

# Discussion

## X in UE\_ID based subgrouping

In RAN2#129bis meeting, the following agreements were achieved:

|  |
| --- |
| * LP-WUS is supported with eDRX, FFS on exact impact if any * Use 5G-S-TMSI to determine the UE\_ID in the formula of UE\_ID based subgrouping for LP-WUS, i.e., UE\_ID=5G-S-TMSI mod X. * X is based on 32 subgrouping number. Details can be discussed in the running CR. |

Then the formula of subgroup ID of UE\_ID based subgrouping for LP-WUS is:

|  |
| --- |
| SubgroupID = (floor(UE\_ID/(N\*Ns\*Np)) mod lp-SubgroupsNumForUEID) + (lp-SubgroupsNumPerPO – lp-SubgroupsNumForUEID),  where:  N: number of total paging frames in T, which is the DRX cycle of RRC\_IDLE state as specified in clause 7.1  Ns: number of paging occasions for a PF  Np is the number of subgroupsNumForUEID for PEI, if configured and UE supports PEI; otherwise, Np is 1  UE\_ID: 5G-S-TMSI mod X, X is FFS  lp-SubgroupsNumForUEID and lp-SubgroupsNumPerPO are the subgroup number for UE\_ID based subgrouping for LP-WUS and the total subgroup number for LP-WUS, respectively. |

The UE-ID value range for UE-ID based subgrouping for LP-WUS depends on the maximum number of POs, the maximum number of UE-ID based PEI sub-groups and the maximum number of UE-ID based subgroups for LP-WUS. And we have already agreed to support LP-WUS with eDRX and consider 32 as the maximum number of UE-ID based subgroups for LP-WUS for X. Therefore, the possible options for X include:

* **Option 1: X is depended on if eDRX is applied and different cases of Np.**

If eDRX is not applied and Np is the number of subgroupsNumForUEID for PEI, X=262144 (256\*4\*8\*32);

If eDRX is not applied and Np is 1, X=32768 (256\*4\*32);

If eDRX is applied and Np is the number of subgroupsNumForUEID for PEI, X=1048576(1024\*4\*8\*32);

If eDRX is applied and Np is 1, X=131072(1024\*4\*32).

* **Option 2: X is depended on if eDRX is applied without considering different cases of Np**

If eDRX is not applied, X=262144 (256\*4\*8\*32);

If eDRX is applied, X= 1048576 (1024\*4\*8\*32).

* **Option 3: X is 1048576, i.e., the largest UE ID range in all LP\_WUS cases is be used for all LP-WUS monitoring cases.**

Companies are invited to provide their preference on above options.

**Q: Which option is preferred for X in the formula of subgroup ID of UE\_ID based subgrouping for LP-WUS?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Preferred option** | **Comments** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Summary:**

## Comments on TS 38.304 running CR

Companies can provide comments and suggestions to the uploaded running CR in this table. Please do not add changes, suggestions, or comments directly to the draft CR document.

|  |  |  |
| --- | --- | --- |
| Company + Issue Number (e.g., C001) | Detailed comments | Rapporteur response |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

## Open issue list

Beside FFS X for UE\_ID in sub-clause 2.1, followings are the Editor’s NOTE in the running CR:

Editor’s NOTE: FFS on the terminology LP-WUS UE.

Editor’s NOTE: Will introduce new parameters for RRM measurement relaxation and offloading according to RRC specification.

Editor’s NOTE: FFS (if needed) on enhancements based on R16 criteria (e.g., based on the LR measurements) for the case when MR serving cell measurement results are not available.

Editor’s NOTE: FFS on exit condition for serving cell RRM relaxation, e.g., whether a separate exit condition other than ‘not fulfilling the entry condition’ is needed, or whether exit condition include MR and/or LR-based measurements.

Editor’s NOTE: The detailed parameters for RRM measurement relaxation for LP-WUS will be aligned with RRC specification.

Editor’s NOTE: FFS how to capture separate thresholds for different UE types (to be aligned with RRC specification).

Editor’s NOTE: FFS relaxed measurement criteria is different from LP-WUS monitoring entry criteria.

Editor’s NOTE: The detailed parameters for serving cell measurement offloading will be aligned with RRC specification.

Editor’s NOTE: FFS if entry/exit conditions are always configured.

Editor’s NOTE: FFS whether/how to capture the mapping between LO and PO. Wait for RAN1 further conclusion on the mapping between LO and PO.

Editor’s NOTE: FFS whether/how to capture the MOs of the LO. Wait for RAN1 further conclusion on MO.

Editor’s NOTE: The detailed calculation for LP-WUS monitoring would be further discussed and decided in RAN1.

Editor’s NOTE: The detailed parameters for LP-WUS monitoring will be aligned with RRC specification.

Editor’s NOTE: FFS how to capture separate entry/exit thresholds for OFDM-based and OOK-based WUR (to be aligned with RRC specification).

Editor’s NOTE: The detailed parameters for LP-WUS monitoring conditions will be aligned with RRC specification.

Editor’s NOTE: The detailed parameters for LP-WUS subgrouping will be aligned with RRC specification.

Editor’s NOTE: The value of a subgroup ID will be aligned with RRC specification.

Editor’s NOTE: The detailed parameters for LP-WUS subgrouping will be aligned with RRC specification.

Among these ENs, the following open issues can be discussed in RAN2, including:

1. FFS on the terminology LP-WUS UE.
2. FFS (if needed) on enhancements based on R16 criteria (e.g., based on the LR measurements) for the case when MR serving cell measurement results are not available.
3. FFS on exit condition for serving cell RRM relaxation, e.g., whether a separate exit condition other than ‘not fulfilling the entry condition’ is needed, or whether exit condition include MR and/or LR-based measurements.
4. FFS relaxed measurement criteria is different from LP-WUS monitoring entry criteria.
5. FFS if entry/exit conditions are always configured.

In addition to the above open issues, please provide your comments on any other RAN2 open issues of 38.304 running CR for LP-WUS, and Rapporteur will response.

|  |  |  |
| --- | --- | --- |
| **Company** | **Open issue** | **Rapporteur response** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

# Conclusion