**3GPP TSG-RAN2 Meeting #129bisR2-25xxxxx**

**Wuhan, China, April 7– 11, 2025**

|  |
| --- |
| *CR-Form-v12.3* |
| **CHANGE REQUEST** |
|  |
|  | **36.331** | **CR** | **5065** | **rev** | **4** | **Current version:** | **18.4.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network | **X** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Introduction of LTE TN to NR NTN IDLE mode mobility |
|  |  |
| ***Source to WG:*** | CATT |
| ***Source to TSG:*** | R2 |
|  |  |
| ***Work item code:*** | LTE\_TN\_NR\_NTN\_mob-Core |  | ***Date:*** | 2025-04-14 |
|  |  |  |  |  |
| ***Category:*** |  |  | ***Release:*** | Rel-19 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19) Rel-20 (Release 20)* |
|  |  |
| ***Reason for change:*** | Introduce Rel-19 LTE TN to NR NTN IDLE mode mobility feature into the Spec. |
|  |  |
| ***Summary of change:*** | The changes are made on the related procedure and siganlling to capture the following agreements made by RAN2:

|  |
| --- |
| RAN2#125bis:Agreement:1. For idle mode mobility from LTE to NR NTN, at least normal LTE UE are in scope. Can come back in the next meeting to check if also eMTC UE and NB-IoT UEs could also be considered in scopeWorking Assumption:2. We don’t introduce multiple SMTCs in LTE |

|  |
| --- |
| RAN2#126:Agreements:1. For idle mode mobility from EUTRA TN to NR NTN, NB-IoT UEs are considered not in the scope.2. For idle mode mobility from EUTRA TN to NR NTN, we don’t consider specific optimizations for BL UEs and UEs in CE.3. SIB24 is reused to provide the NR NTN cell reselection related information (e.g. frequency information, SMTC config, etc.), introducing a satellite ID list in per frequency. The EUTRA cell provides the satellite assistance information for NR neighbor cell per satellite, as identified by the satellite ID. 4. To support the idle mode mobility from EUTRA TN to NR NTN, the satellite assistance information for NR NTN neighbor cells is needed and should include the following parameters: - Satellite ephemeris information - TA common information - k-Mac - epoch time - validity duration - ntn-PolarizationDL (FFS if mandatory or optional)5. The Ephemeris information/epoch time/k-mac/validity duration IEs defined in SIB33 specified in TS36.331 should be reused for NR satellite assistance information.6. The signalling format for ntn-PolarizationDL and TA common related configurations within NTN-Config specified in TS38.331 should be introduced in TS36.331 for NR satellite assistance information.7. RAN2 will decide in the next meeting which of the following options to adopt for the provision of the NR satellite assistance information (based on TPs provided by the WI RRC Rapporteur): Option 1: Introduce a new SIB to include the NR satellite assistance information. Option 2: Define new IE for NR satellite assistance information and define separate neighbour satellite information list to provide the NR satellite information in SIB33. Option 3: Extend the NeighSatelliteInfo defined for IoT NTN to include the parameters needed for NR satellite, and reuse the neighSatelliteInfoList defined in SIB33 to provide either NR or IoT NTN information.8. Introduce the clarification in the field description of measTimingConfig (configured via SIB24 in TS 36.331) that it is configured based on the assumption that the gNB-UE propagation delay equals to 0 ms, and UE can adjust the offset based on the actual propagation delay, when the corresponding frequency is associated with a satellite ID.Working Assumption: 1. NR NTN cell reselection evaluation is based on RRM measurements as legacy; no spec impact foreseen for EUTRA TN to NR NTN cell (can come back in the next meeting to see if the WA can be confirmed) |

|  |
| --- |
| RAN2#127:Agreements:1. Define new IE for NR satellite assistance information and define separate neighbour satellite information list to provide the NR satellite information in SIB33.2. The ntn-PolarizationalDL is optional.3. Reuse the SatelliteId-r18 to identify either an NR satellite or an IoT NTN satellite4. Consider a solution that avoids repeating the ephemeris for a satellite which provides both IoT NTN and NR NTN cells 5. maxSat-r17 (4) is reused for the maximum number of NR satellites.6. RAN2 will not do further work to introduce multiple SMTCs in LTE7. NR NTN cell reselection evaluation is based on RRM measurements as legacy; no spec impact foreseen for EUTRA TN to NR NTN cell.8. RAN2 confirms that measurements of NR NTN cells for a UE in E-UTRAN TN RRC\_INACTIVE are supported, with the understanding that UE moves to RRC idle upon selecting the NR NTN cell 9. Introduce a new UE capability without signalling for LTE TN to NR NTN mobility. |

|  |
| --- |
| RAN2#127bis:Agreements:1. The following signalling design is agreed, to avoid ephemeris duplication for the same satellite providing both IoT NTN and NR NTN: The satelliteId-r19 in an entry of NR NTN assistance info list (i.e. neighSatelliteInfoListNR) can be set equal to a Satellite ID value included in IoT NTN assistance info list (i.e. neighSatelliteInfoList) and thus refers to the ephemeris data of IoT NTN identified by this specific Satellite ID, in which case the ephemeris data (i.e. ephemerisInfo-r19) in that entry of neighSatelliteInfoListNR can be absent. 2. Regarding satellite ID assignment across IoT NTN and NR NTN satellite assistance info lists, RAN2 thinks this can be left to NW implementation to handle.3. RAN2 sticks to the agreement that only duplication of ephemeris data needs to be avoided in the case of same satellite supporting both NR NTN and IoT NTN. |

|  |
| --- |
| RAN2#128:Agreements:1. RAN2 understands that the UE behaviour is currently not clear if the network includes a NR NTN frequency in redirectedCarrierInfo in the RRCConnectionRelease message in a TN cell. We can further discuss whether we want to clarify the UE behaviour and in case whether we need to introduce a new UE capability.2. Add a clarification in Stage 2 that only LTE to NR NTN is supported (and not eMTC NTN to NR NTN). Also add in the field description that NeighSatelliteInfoNR-r19 is only signalled in a LTE TN cell but not IoT NTN cell. |

|  |
| --- |
| RAN2#129:Agreements:1. RAN2 confirms that redirection from LTE TN to NR NTN is not supported before Rel-19.2. Redirection from LTE TN to NR NTN is supported in Rel-19 introducing a new capability signaling for LTE TN to NR NTN redirection purpose and also a satellite ID(s) in RedirectedCarrierInfo. |

|  |
| --- |
| RAN2 129bis:Agreements:1. RAN2 confirms that redirection from LTE TN to NR NTN is not supported before Rel-19.2. Extend the capability signaling for E-UTRA TN to NR NTN redirection to also indicate the support of IRAT E-UTRA TN to NR NTN cell reselection. E-UTRAN that broadcasts NR satellite assistance info in SIB33 may configure dedicated priority for an NR NTN frequency, only if it receives this capability common to E-UTRA TN to NR NTN redirection and cell reselection (based on NW implementation).3. The redirection to NR NTN information element is enclosed in an NTN specific CarrierInfoNR, which is introduced in the choice structure as nr-19. |

 |
|  |  |
| ***Consequences if not approved:*** | Rel-19 feature LTE TN to NR NTN IDLE mode mobility is not supported in the specifications. |
|  |  |
| ***Clauses affected:*** | 3.1, 5.2.2.3, 6.2.2, 6.3.1, 6.3.4, 6.3.6, 6.4 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** | **X** |  |  Other core specifications  | TS/TR 36.300 CR 1412TS/TR 36.306 CR 1900 |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

|  |
| --- |
| Start of change |

## 3.1 Definitions

For the purposes of the present document, the terms and definitions given in TR 21.905 [1] and the following apply. A term defined in the present document takes precedence over the definition of the same term, if any, in TR 21.905 [1].

**A2X communication**: A communication to support A2X services leveraging PC5 reference points, as defined in TS 23.256 [115]. A2X services are realized by various types of A2X applications, e.g., BRID or DAA.

**Aerial UE:** UE performing Aerial UE communication, as defined in TS 36.300 [9], clause 23.17 and TS 23.256 [115].

**Anchor carrier:** In NB-IoT, a carrier where the UE assumes that NPSS/NSSS/NPBCH/SIB-NB for FDD or NPSS/NSSS/NPBCH for TDD are transmitted.

**Bandwidth Reduced:** Refers to operation in downlink and uplink with a limited channel bandwidth of 6 PRBs.

**CEIL:** Mathematical function used to 'round up' i.e. to the nearest integer having a higher or equal value.

**Cellular IoT EPS Optimisation**: Provides improved support of small data transfer, as defined in TS 24.301 [35].

**Commercial Mobile Alert System:** Public Warning System that delivers *Warning Notifications* provided by *Warning Notification Providers* to CMAS capable UEs.

**Common access barring parameters:** The common access barring parameters refer to the access class barring parameters that are broadcast in *SystemInformationBlockType2* outside the list of PLMN specific parameters (i.e. in *ac-BarringPerPLMN-List*).

**Control plane CIoT 5GS optimisation:** Enables support of efficient transport of user data (IP, Ethernet or unstructured) or SMS messages over control plane via the AMF without triggering data radio bearer establishment, as defined in TS 24.501 [95].

**Control plane CIoT EPS optimisation**: Enables support of efficient transport of user data (IP, non-IP or SMS) over control plane via the MME without triggering data radio bearer establishment, as defined in TS 24.301 [35].

**Control plane EDT**: Early Data Transmission used with the Control plane CIoT EPS optimisation or Control plane CIoT 5GS optimisation.

**Coverage-based paging**: In NB-IoT allows UE to use paging carriers configured for lower levels of coverage enhancement than maximum coverage enhancement supported in the cell as described in TS 36.300 [9].

**CSG member cell:** A cell broadcasting the identity of the selected PLMN, registered PLMN or equivalent PLMN and for which the Permitted CSG list of the UE includes an entry comprising cell's CSG ID and the respective PLMN identity.

**DAPS bearer**: A bearer whose radio protocols are located in both the source eNB and the target eNB during a DAPS handover to use both source eNB and target eNB resources.

**Dual Connectivity**: A UE in RRC\_CONNECTED is configured with Dual Connectivity when configured with a Master and a Secondary Cell Group.

**Early Data Transmission:** Allows one uplink data transmission optionally followed by one downlink data transmission during the random access procedure as specified in TS 36.300 [9]. The S1 connection is established or resumed upon reception of the uplink data and may be released or suspended along with the transmission of the downlink data. Early data transmission refers to both CP-EDT and UP-EDT.

**Early Security Reactivation:** Re-activation of AS security prior to the transmission of *RRCConnectionResumeRequest* message when a UE is provided with an NCC value during suspension.

**Earth-moving cell**: An NTN cell moving on the ground. It can be provisioned by beam(s) whose coverage area slides over the Earth's surface (e.g., the case of NGSO satellites generating fixed or non-steerable beams).

**Ephemeris:** A set of parameters that describe the movement of an NTN node over time.

**E-UTRA-NR Dual Connectivity:** A form of dual connectivity in which a UE in RRC\_CONNECTED is configured with MCG cells using E-UTRA and SCG cells using NR as defined in TS 37.340 [81].

**EU-Alert:** Public Warning System that delivers Warning Notifications provided by Warning Notification Providers using the same AS mechanisms as defined for CMAS.

**Field:** The individual contents of an information element are referred as fields.

**FLOOR:** Mathematical function used to 'round down' i.e. to the nearest integer having a lower or equal value.

**FR1:** Frequency range 1 as defined in clause 5.1 of TS 38.101-1 [85].

**FR2:** Frequency range 2 as defined in clause 5.1 of TS 38.101-2 [100].

**Geosynchronous Orbit:** Earth-centred orbit at approximately 35,786 kilometres in altitude above Earth's surface and synchronised with Earth's rotation. A geostationary orbit is a non-inclined geosynchronous orbit, i.e. in the Earth's equator plane.

**Information element:** A structural element containing a single or multiple fields is referred as information element.

**Korean Public Alert System (KPAS):** Public Warning System that delivers Warning Notifications provided by Warning Notification Providers using the same AS mechanisms as defined for CMAS.

**Master Cell Group**: For a UE not configured with DC, the MCG comprises all serving cells. For a UE configured with DC, the MCG concerns a subset of the serving cells comprising of the PCell and zero or more secondary cells.

**Mixed Operation Mode:** In NB-IoT FDD, multi-carrier operation where the anchor carrier is in standalone mode while the non-anchor carrier is in inband or guardand mode, and vice versa. See TS 36.300 [9].

**MBMS service:** MBMS bearer service as defined in TS 23.246 [56] (i.e. provided via an MRB or an SC-MRB).

**NB-IoT:** NB-IoT allows access to network services via E-UTRA with a channel bandwidth limited to 200 kHz.

**NB-IoT UE:** A UE that uses NB-IoT.

**NCSG:** Network controlled small gap as defined in TS 36.133 [16].

**Non-geosynchronous orbit:** Earth-centred orbit with an orbital period that does not match Earth's rotation on its axis. This includes Low Earth Orbit (LEO) and Medium Earth Orbit (MEO).

**Non-terrestrial networks:** An E-UTRAN consisting of eNBs, which provide non-terrestrial LTE access to UEs by means of an NTN payload embarked on a space-borne NTN vehicle and an NTN Gateway.

**NR-E-UTRA Dual Connectivity (NE-DC):** A form of dual connectivity in which a UE in RRC\_CONNECTED is configured with MCG cells using NR and SCG cells using E-UTRA as defined in TS 37.340 [81].

**Non-anchor carrier:** In NB-IoT, a carrier where the UE does not assume that NPSS/NSSS/NPBCH/SIB-NB for FDD or NPSS/NSSS/NPBCH for TDD are transmitted.

**NR Carrier Frequency:** Frequency referring to the position of resource element RE=#0 (subcarrier #0) of resource block RB#10 of the SS block.

**NR NTN:** an NG-RAN consisting of gNBs, which provide non-terrestrial NR access to UEs by means of an NTN payload embarked on an airborne and space-borne NTN vehicle and an NTN Gateway.

**NR sidelink communication**: AS functionality enabling at least V2X Communication as defined in TS 23.287 [104] and/or A2X Communication as defined in TS 23.256 [115], between two or more nearby UEs, using NR technology but not traversing any network node.

**Primary Cell**: The cell, operating on the primary frequency, in which the UE either performs the initial connection establishment procedure or initiates the connection re-establishment procedure, or the cell indicated as the primary cell in the handover procedure.

**Primary Secondary Cell**: The SCG cell in which the UE is instructed to perform random access or initial PUSCH transmission if random access procedure is skipped when performing the SCG change procedure.

**Primary Timing Advance Group**: Timing Advance Group containing the PCell or the PSCell.

**PUCCH SCell:** An SCell configured with PUCCH.

**Quasi-earth fixed cell:** An NTN cell fixed with respect to a certain geographic area on the earth during a certain time duration. This can be provided by beam(s) covering one geographic area for a finite period and a different geographic area during another period (e.g., the case of NGSO satellites generating steerable beams).

**RLC bearer configuration:** The lower layer part of the radio bearer configuration comprising the RLC and logical channel configurations.

**Satellite:** A space-borne vehicle orbiting the Earth that carries the NTN payload.

**Secondary Cell**: A cell, operating on a secondary frequency, which may be configured once an RRC connection is established and which may be used to provide additional radio resources. Except for the case of (NG)EN-DC, the PSCell is considered to be an SCell.

**Secondary Cell Group**: For a UE configured with DC, the subset of serving cells not part of the MCG, i.e. comprising of the PSCell and zero or more other secondary cells.

**Secondary Timing Advance Group**: Timing Advance Group neither containing the PCell nor the PSCell. A secondary timing advance group contains at least one cell with configured uplink.

**Serving Cell**: For a UE in RRC\_CONNECTED not configured with CA/ DC there is only one serving cell comprising of the primary cell. For a UE in RRC\_CONNECTED configured with CA/ DC the term 'serving cells' is used to denote the set of one or more cells comprising of the primary cell and all secondary cells.

**Sidelink**: UE to UE interface for sidelink communication, V2X sidelink communication, A2X sidelink communication and sidelink discovery. The sidelink corresponds to the PC5 interface as defined in TS 23.303 [68].

**Sidelink communication**: AS functionality enabling ProSe Direct Communication as defined in TS 23.303 [68], between two or more nearby UEs, using E-UTRA technology but not traversing any network node. In this version, the terminology "sidelink communication" without "V2X" or "A2X" prefix only concerns PS unless specifically stated otherwise.

**Sidelink discovery**: AS functionality enabling ProSe Direct Discovery as defined in TS 23.303 [68], using E-UTRA technology but not traversing any network node.

**Sidelink operation**: Includes sidelink communication, V2X sidelink communication, A2X sidelink communication and sidelink discovery.

**Split SRB**: in MR-DC, an SRB between the MN and the UE, allowing selection of either the direct path or the path via the SN as well as duplication of RRC PDUs across both paths as defined in TS 37.340 [81].

**Timing Advance Group**: A group of serving cells that is configured by RRC and that, for the cells with an UL configured, use the same timing reference cell and the same Timing Advance value. A Timing Advance Group only includes cells of the same cell group i.e. it either includes MCG cells or SCG cells.

**Transmission using PUR:** Allows one uplink data transmission using preconfigured uplink resource from RRC\_IDLE mode as specified in TS 36.300 [9]. Transmission using PUR refers to both CP transmission using PUR and UP transmission using PUR.

**UE Inactive AS Context:** UE Inactive AS Context is stored when the connection is suspended and restored when the connection is resumed. It includes information as defined in clause 5.3.8.7.

**UE in CE:** Refers to a UE that is capable of using coverage enhancement, and requires coverage enhancement mode to access a cell or is configured in a coverage enhancement mode.

**User plane CIoT 5GS optimisation:** Enables support for change from 5GMM-IDLE mode to 5GMM-CONNECTED mode without the need for using the Service Request procedure, as defined in TS 24.501 [95].

**User plane CIoT EPS optimisation**: Enables support for change from EMM-IDLE mode to EMM-CONNECTED mode without the need for using the Service Request procedure, as defined in TS 24.301 [35].

**User plane EDT:** Early Data Transmission used with the User plane CIoT EPS optimisation or User plane CIoT 5GS optimisation.

**V2X sidelink communication**: AS functionality enabling V2X Communication as defined in TS 23.285 [78], between nearby UEs, using E-UTRA technology but not traversing any network node.

|  |
| --- |
| Next change |

#### 5.2.2.3 System information required by the UE

The UE shall:

1> ensure having a valid version, as defined below, of (at least) the following system information, also referred to as the 'required' system information:

2> if in RRC\_IDLE:

3> if the UE is a NB-IoT UE:

4> the *MasterInformationBlock-NB/ MasterInformationBlock-TDD-NB* and *SystemInformationBlockType1-NB* as well as *SystemInformationBlockType2-NB* through *SystemInformationBlockType5-NB, SystemInformationBlockType22-NB*;

3> else:

4> the *MasterInformationBlock* and *SystemInformationBlockType1* (or *SystemInformationBlockType1-BR* depending on whether the UE is a BL UE or the UE in CE) as well as *SystemInformationBlockType2* through *SystemInformationBlockType8* and *SystemInformationBlockType24* (depending on support of the concerned RATs), *SystemInformationBlockType17* (depending on support of RAN-assisted WLAN interworking when the UE is connected to EPC), *SystemInformationBlockType25* (depending on support of E-UTRA/5GC), *SystemInformationBlockType29* (only for BL UE or the UE in CE depending on support of resource reservation), *SystemInformationBlockType21*, *SystemInformationBlockType26* (if UE is capable of V2X sidelink communication and is configured by upper layers to receive or transmit V2X sidelink communication),and *SystemInformationBlockType28* (if UE is capable of NR sidelink communication and is configured by upper layers to receive or transmit NR sidelink communication), *SystemInformationBlockType30* (if UE is configured by upper layers to report disaster roaming related information);

3> if initiating a RRC connection establishment/resume procedure; and

3> the UE is NTN capable:

4> *SystemInformationBlockType31* (*SystemInformationBlockType31-NB* in NB-IoT),if scheduled;

2> if in RRC\_INACTIVE:

3> the *MasterInformationBlock* and *SystemInformationBlockType1* as well as *SystemInformationBlockType2* through *SystemInformationBlockType8* (depending on support of the concerned RATs), *SystemInformationBlockType24* (depending on support of the concerned RATs), *SystemInformationBlockType25*, *SystemInformationBlockType29* (only for BL UE or the UE in CE depending on support of resource reservation), *SystemInformationBlockType21*, *SystemInformationBlockType26* (if UE is capable of V2X sidelink communication and is configured by upper layers to receive or transmit V2X sidelink communication),and *SystemInformationBlockType28* (if UE is capable of NR sidelink communication and is configured by upper layers to receive or transmit NR sidelink communication), *SystemInformationBlockType30* (if UE is configured by upper layers to report disaster roaming related information);

2> if in RRC\_CONNECTED; and

2> the UE is not a BL UE; and

2> the UE is not in CE; and

2> the UE is not a NB-IoT UE:

3> the *MasterInformationBlock*, *SystemInformationBlockType1* and *SystemInformationBlockType2* as well as *SystemInformationBlockType8* (depending on support of CDMA2000), *SystemInformationBlockType17* (depending on support of RAN-assisted WLAN interworking when the UE is connected to EPC), *SystemInformationBlockType25* (depending on support of E-UTRA/5GC);

2> if in RRC\_CONNECTED and T311 is running; and

2> the UE is a BL UE or the UE is in CE or the UE is a NB-IoT UE:

3> the *MasterInformationBlock* (or *MasterInformationBlock-NB/ MasterInformationBlock-TDD-NB* in NB-IoT), *SystemInformationBlockType1-BR* (or *SystemInformationBlockType1-NB* in NB-IoT) and *SystemInformationBlockType2* (or *SystemInformationBlockType2-NB* in NB-IoT), *SystemInformationBlockType25* (only for BL UE or the UE in CE depending on support of E-UTRA/5GC), *SystemInformationBlockType29* (only for BL UE or the UE in CE depending on support of resource reservation), *SystemInformationBlockType31* (*SystemInformationBlockType31-NB* in NB-IoT) (only for NTN capable UE) if scheduled, and for NB-IoT *SystemInformationBlockType22-NB*;

2> if in RRC\_CONNECTED and T317 is not running; and

2> the UE is NTN capable:

3> *SystemInformationBlockType31* (*SystemInformationBlockType31-NB* in NB-IoT), if scheduled;

1> delete any stored system information after 3 hours or 24 hours from the moment it was confirmed to be valid as defined in 5.2.1.3, unless specified otherwise;

1> consider any stored system information except *SystemInformationBlockType10,* *SystemInformationBlockType11,* *systemInformationBlockType12, systemInformationBlockType14* (*systemInformationBlockType14-NB* in NB-IoT), *systemInformationBlockType25* and *systemInformationBlockType31* (*systemInformationBlockType31-NB* in NB-IoT) and *systemInformationBlockType33*, to be invalid if *systemInfoValueTag* included in the *SystemInformationBlockType1* (*MasterInformationBlock-NB/ MasterInformationBlock-TDD-NB* in NB-IoT) is different from the one of the stored system information and in case of NB-IoT UEs, BL UEs and UEs in CE, *systemInfoValueTagSI* is not broadcasted. Otherwise consider system information validity as defined in 5.2.1.3;

|  |
| --- |
| Next change |

### 6.2.2 Message definitions

<Irrelevant Texts Omitted>

#### – *RRCConnectionRelease*

The *RRCConnectionRelease* message is used to command the release of an RRC connection, or to complete an UP-EDT procedure.

Signalling radio bearer: SRB1

RLC-SAP: AM

Logical channel: DCCH

Direction: E‑UTRAN to UE

*RRCConnectionRelease message*

-- ASN1START

RRCConnectionRelease ::= SEQUENCE {

 rrc-TransactionIdentifier RRC-TransactionIdentifier,

 criticalExtensions CHOICE {

 c1 CHOICE {

 rrcConnectionRelease-r8 RRCConnectionRelease-r8-IEs,

 spare3 NULL, spare2 NULL, spare1 NULL

 },

 criticalExtensionsFuture SEQUENCE {}

 }

}

RRCConnectionRelease-r8-IEs ::= SEQUENCE {

 releaseCause ReleaseCause,

 redirectedCarrierInfo RedirectedCarrierInfo OPTIONAL, -- Need ON

 idleModeMobilityControlInfo IdleModeMobilityControlInfo OPTIONAL, -- Need OP

 nonCriticalExtension RRCConnectionRelease-v890-IEs OPTIONAL

}

RRCConnectionRelease-v890-IEs ::= SEQUENCE {

 lateNonCriticalExtension OCTET STRING (CONTAINING RRCConnectionRelease-v9e0-IEs) OPTIONAL,

 nonCriticalExtension RRCConnectionRelease-v920-IEs OPTIONAL

}

-- Late non critical extensions

RRCConnectionRelease-v9e0-IEs ::= SEQUENCE {

 redirectedCarrierInfo-v9e0 RedirectedCarrierInfo-v9e0 OPTIONAL, -- Cond NoRedirect-r8

 idleModeMobilityControlInfo-v9e0 IdleModeMobilityControlInfo-v9e0 OPTIONAL, -- Cond IdleInfoEUTRA

 nonCriticalExtension SEQUENCE {} OPTIONAL

}

-- Regular non critical extensions

RRCConnectionRelease-v920-IEs ::= SEQUENCE {

 cellInfoList-r9 CHOICE {

 geran-r9 CellInfoListGERAN-r9,

 utra-FDD-r9 CellInfoListUTRA-FDD-r9,

 utra-TDD-r9 CellInfoListUTRA-TDD-r9,

 ...,

 utra-TDD-r10 CellInfoListUTRA-TDD-r10

 } OPTIONAL, -- Cond Redirection

 nonCriticalExtension RRCConnectionRelease-v1020-IEs OPTIONAL

}

RRCConnectionRelease-v1020-IEs ::= SEQUENCE {

 extendedWaitTime-r10 INTEGER (1..1800) OPTIONAL, -- Need ON

 nonCriticalExtension RRCConnectionRelease-v1320-IEs OPTIONAL

}

RRCConnectionRelease-v1320-IEs::= SEQUENCE {

 resumeIdentity-r13 ResumeIdentity-r13 OPTIONAL, -- Need OR

 nonCriticalExtension RRCConnectionRelease-v1530-IEs OPTIONAL

}

RRCConnectionRelease-v1530-IEs ::= SEQUENCE {

 drb-ContinueROHC-r15 ENUMERATED {true} OPTIONAL, -- Cond UP-EDTorPUR

 nextHopChainingCount-r15 NextHopChainingCount OPTIONAL, -- Cond EarlySec

 measIdleConfig-r15 MeasIdleConfigDedicated-r15 OPTIONAL, -- Need ON

 rrc-InactiveConfig-r15 RRC-InactiveConfig-r15 OPTIONAL, -- Need OR

 cn-Type-r15 ENUMERATED {epc,fivegc} OPTIONAL, -- Need OR

 nonCriticalExtension RRCConnectionRelease-v1540-IEs OPTIONAL

}

RRCConnectionRelease-v1540-IEs ::= SEQUENCE {

 waitTime INTEGER (1..16) OPTIONAL, -- Cond 5GC

 nonCriticalExtension RRCConnectionRelease-v15b0-IEs OPTIONAL

}

RRCConnectionRelease-v15b0-IEs ::= SEQUENCE {

 noLastCellUpdate-r15 ENUMERATED {true} OPTIONAL, -- Need OP

 nonCriticalExtension RRCConnectionRelease-v1610-IEs OPTIONAL

}

RRCConnectionRelease-v1610-IEs ::= SEQUENCE {

 fullI-RNTI-r16 I-RNTI-r15 OPTIONAL, -- Need OR

 shortI-RNTI-r16 ShortI-RNTI-r15 OPTIONAL, -- Need OR

 pur-Config-r16 SetupRelease {PUR-Config-r16} OPTIONAL, -- Need ON

 rrc-InactiveConfig-v1610 RRC-InactiveConfig-v1610 OPTIONAL, -- Cond BLCE-IDLEeDRX

 releaseIdleMeasConfig-r16 ENUMERATED {true} OPTIONAL, -- Need ON

 altFreqPriorities-r16 ENUMERATED {true} OPTIONAL, -- Need ON

 t323-r16 ENUMERATED {

 min5, min10, min20, min30, min60, min120, min180,

 min720} OPTIONAL, -- Need OR

 nonCriticalExtension RRCConnectionRelease-v1650-IEs OPTIONAL

}

RRCConnectionRelease-v1650-IEs ::= SEQUENCE {

 mpsPriorityIndication-r16 ENUMERATED {true} OPTIONAL, -- Cond Redirection2

 nonCriticalExtension SEQUENCE {} OPTIONAL

}

ReleaseCause ::= ENUMERATED {loadBalancingTAUrequired,

 other, cs-FallbackHighPriority-v1020, rrc-Suspend-v1320}

RedirectedCarrierInfo ::= CHOICE {

 eutra ARFCN-ValueEUTRA,

 geran CarrierFreqsGERAN,

 utra-FDD ARFCN-ValueUTRA,

 utra-TDD ARFCN-ValueUTRA,

 cdma2000-HRPD CarrierFreqCDMA2000,

 cdma2000-1xRTT CarrierFreqCDMA2000,

 ...,

 utra-TDD-r10 CarrierFreqListUTRA-TDD-r10,

 nr-r15 CarrierInfoNR-r15,

 nr-r17 CarrierInfoNR-r17,

 nr-r19 CarrierInfoNR-r19

}

RedirectedCarrierInfo-v9e0 ::= SEQUENCE {

 eutra-v9e0 ARFCN-ValueEUTRA-v9e0

}

RRC-InactiveConfig-r15::= SEQUENCE {

 fullI-RNTI-r15 I-RNTI-r15,

 shortI-RNTI-r15 ShortI-RNTI-r15,

 ran-PagingCycle-r15 ENUMERATED { rf32, rf64, rf128, rf256} OPTIONAL, --Need OR

 ran-NotificationAreaInfo-r15 RAN-NotificationAreaInfo-r15 OPTIONAL, --Need ON

 periodic-RNAU-timer-r15 ENUMERATED {min5, min10, min20, min30, min60,

 min120, min360, min720} OPTIONAL, --Need OR

 nextHopChainingCount-r15 NextHopChainingCount OPTIONAL, --Cond INACTIVE

 dummy SEQUENCE{} OPTIONAL

}

RRC-InactiveConfig-v1610::= SEQUENCE {

 ran-PagingCycle-v1610 ENUMERATED {rf512, rf1024}

}

RAN-NotificationAreaInfo-r15 ::= CHOICE {

 cellList PLMN-RAN-AreaCellList-r15,

 ran-AreaConfigList PLMN-RAN-AreaConfigList-r15

}

PLMN-RAN-AreaCellList-r15 ::= SEQUENCE (SIZE (1..maxPLMN-r15)) OF PLMN-RAN-AreaCell-r15

PLMN-RAN-AreaCell-r15 ::= SEQUENCE {

 plmn-Identity-r15 PLMN-Identity OPTIONAL,

 ran-AreaCells-r15 SEQUENCE (SIZE (1..32)) OF CellIdentity

}

PLMN-RAN-AreaConfigList-r15 ::= SEQUENCE (SIZE (1..maxPLMN-r15)) OF PLMN-RAN-AreaConfig-r15

PLMN-RAN-AreaConfig-r15 ::= SEQUENCE {

 plmn-Identity-r15 PLMN-Identity OPTIONAL,

 ran-Area-r15 SEQUENCE (SIZE (1..16)) OF RAN-AreaConfig-r15

}

RAN-AreaConfig-r15 ::= SEQUENCE {

 trackingAreaCode-5GC-r15 TrackingAreaCode-5GC-r15,

 ran-AreaCodeList-r15 SEQUENCE (SIZE (1..32)) OF RAN-AreaCode-r15 OPTIONAL --Need OR

}

CarrierFreqListUTRA-TDD-r10 ::= SEQUENCE (SIZE (1..maxFreqUTRA-TDD-r10)) OF ARFCN-ValueUTRA

IdleModeMobilityControlInfo ::= SEQUENCE {

 freqPriorityListEUTRA FreqPriorityListEUTRA OPTIONAL, -- Need ON

 freqPriorityListGERAN FreqsPriorityListGERAN OPTIONAL, -- Need ON

 freqPriorityListUTRA-FDD FreqPriorityListUTRA-FDD OPTIONAL, -- Need ON

 freqPriorityListUTRA-TDD FreqPriorityListUTRA-TDD OPTIONAL, -- Need ON

 bandClassPriorityListHRPD BandClassPriorityListHRPD OPTIONAL, -- Need ON

 bandClassPriorityList1XRTT BandClassPriorityList1XRTT OPTIONAL, -- Need ON

 t320 ENUMERATED {

 min5, min10, min20, min30, min60, min120, min180,

 spare1} OPTIONAL, -- Need OR

 ...,

 [[ freqPriorityListExtEUTRA-r12 FreqPriorityListExtEUTRA-r12 OPTIONAL -- Need ON

 ]],

 [[ freqPriorityListEUTRA-v1310 FreqPriorityListEUTRA-v1310 OPTIONAL, -- Need ON

 freqPriorityListExtEUTRA-v1310 FreqPriorityListExtEUTRA-v1310 OPTIONAL -- Need ON

 ]],

 [[ freqPriorityListNR-r15 FreqPriorityListNR-r15 OPTIONAL -- Need ON

 ]]

}

IdleModeMobilityControlInfo-v9e0 ::= SEQUENCE {

 freqPriorityListEUTRA-v9e0 SEQUENCE (SIZE (1..maxFreq)) OF FreqPriorityEUTRA-v9e0

}

FreqPriorityListEUTRA ::= SEQUENCE (SIZE (1..maxFreq)) OF FreqPriorityEUTRA

FreqPriorityListExtEUTRA-r12 ::= SEQUENCE (SIZE (1..maxFreq)) OF FreqPriorityEUTRA-r12

FreqPriorityListEUTRA-v1310 ::= SEQUENCE (SIZE (1..maxFreq)) OF FreqPriorityEUTRA-v1310

FreqPriorityListExtEUTRA-v1310 ::= SEQUENCE (SIZE (1..maxFreq)) OF FreqPriorityEUTRA-v1310

FreqPriorityEUTRA ::= SEQUENCE {

 carrierFreq ARFCN-ValueEUTRA,

 cellReselectionPriority CellReselectionPriority

}

FreqPriorityEUTRA-v9e0 ::= SEQUENCE {

 carrierFreq-v9e0 ARFCN-ValueEUTRA-v9e0 OPTIONAL -- Cond EARFCN-max

}

FreqPriorityEUTRA-r12 ::= SEQUENCE {

 carrierFreq-r12 ARFCN-ValueEUTRA-r9,

 cellReselectionPriority-r12 CellReselectionPriority

}

FreqPriorityEUTRA-v1310 ::= SEQUENCE {

 cellReselectionSubPriority-r13 CellReselectionSubPriority-r13 OPTIONAL -- Need ON

}

FreqPriorityListNR-r15 ::= SEQUENCE (SIZE (1..maxFreq)) OF FreqPriorityNR-r15

FreqPriorityNR-r15 ::= SEQUENCE {

 carrierFreq-r15 ARFCN-ValueNR-r15,

 cellReselectionPriority-r15 CellReselectionPriority,

 cellReselectionSubPriority-r15 CellReselectionSubPriority-r13 OPTIONAL -- Need OR

}

FreqsPriorityListGERAN ::= SEQUENCE (SIZE (1..maxGNFG)) OF FreqsPriorityGERAN

FreqsPriorityGERAN ::= SEQUENCE {

 carrierFreqs CarrierFreqsGERAN,

 cellReselectionPriority CellReselectionPriority

}

FreqPriorityListUTRA-FDD ::= SEQUENCE (SIZE (1..maxUTRA-FDD-Carrier)) OF FreqPriorityUTRA-FDD

FreqPriorityUTRA-FDD ::= SEQUENCE {

 carrierFreq ARFCN-ValueUTRA,

 cellReselectionPriority CellReselectionPriority

}

FreqPriorityListUTRA-TDD ::= SEQUENCE (SIZE (1..maxUTRA-TDD-Carrier)) OF FreqPriorityUTRA-TDD

FreqPriorityUTRA-TDD ::= SEQUENCE {

 carrierFreq ARFCN-ValueUTRA,

 cellReselectionPriority CellReselectionPriority

}

BandClassPriorityListHRPD ::= SEQUENCE (SIZE (1..maxCDMA-BandClass)) OF BandClassPriorityHRPD

BandClassPriorityHRPD ::= SEQUENCE {

 bandClass BandclassCDMA2000,

 cellReselectionPriority CellReselectionPriority

}

BandClassPriorityList1XRTT ::= SEQUENCE (SIZE (1..maxCDMA-BandClass)) OF BandClassPriority1XRTT

BandClassPriority1XRTT ::= SEQUENCE {

 bandClass BandclassCDMA2000,

 cellReselectionPriority CellReselectionPriority

}

CellInfoListGERAN-r9 ::= SEQUENCE (SIZE (1..maxCellInfoGERAN-r9)) OF CellInfoGERAN-r9

CellInfoGERAN-r9 ::= SEQUENCE {

 physCellId-r9 PhysCellIdGERAN,

 carrierFreq-r9 CarrierFreqGERAN,

 systemInformation-r9 SystemInfoListGERAN

}

CarrierInfoNR-r15 ::= SEQUENCE {

 carrierFreq-r15 ARFCN-ValueNR-r15,

 subcarrierSpacingSSB-r15 ENUMERATED {kHz15, kHz30, kHz120, kHz240},

 smtc-r15 MTC-SSB-NR-r15 OPTIONAL -- Need OP

}

CarrierInfoNR-r17 ::= SEQUENCE {

 carrierFreq-r17 ARFCN-ValueNR-r15,

 subcarrierSpacingSSB-r17 ENUMERATED {kHz15, kHz30, kHz120, kHz240, kHz480, spare1},

 smtc-r17 MTC-SSB-NR-r15 OPTIONAL -- Need OP

}

CarrierInfoNR-r19 ::= SEQUENCE {

 carrierFreq-r19 ARFCN-ValueNR-r15,

 subcarrierSpacingSSB-r19 ENUMERATED {kHz15, kHz30, kHz120, kHz240},

 smtc-r19 MTC-SSB-NR-r15 OPTIONAL, -- Need OP

 satAssistanceInfoList-r19 SEQUENCE (SIZE(1..maxSat-r17)) OF SatelliteId-r18

}

CellInfoListUTRA-FDD-r9 ::= SEQUENCE (SIZE (1..maxCellInfoUTRA-r9)) OF CellInfoUTRA-FDD-r9

CellInfoUTRA-FDD-r9 ::= SEQUENCE {

 physCellId-r9 PhysCellIdUTRA-FDD,

 utra-BCCH-Container-r9 OCTET STRING

}

CellInfoListUTRA-TDD-r9 ::= SEQUENCE (SIZE (1..maxCellInfoUTRA-r9)) OF CellInfoUTRA-TDD-r9

CellInfoUTRA-TDD-r9 ::= SEQUENCE {

 physCellId-r9 PhysCellIdUTRA-TDD,

 utra-BCCH-Container-r9 OCTET STRING

}

CellInfoListUTRA-TDD-r10 ::= SEQUENCE (SIZE (1..maxCellInfoUTRA-r9)) OF CellInfoUTRA-TDD-r10

CellInfoUTRA-TDD-r10 ::= SEQUENCE {

 physCellId-r10 PhysCellIdUTRA-TDD,

 carrierFreq-r10 ARFCN-ValueUTRA,

 utra-BCCH-Container-r10 OCTET STRING

}

-- ASN1STOP

| *RRCConnectionRelease* field descriptions |
| --- |
| ***altFreqPriorities***Indicates that the UE shall apply the alternative cell reselectionpriorities, when available. This field is not configured together with *idleModeMobilityControlInfo*. |
| ***carrierFreq or bandClass***The carrier frequency (UTRA, E-UTRA, and NR) and band class (HRPD and 1xRTT) for which the associated cellReselectionPriority is applied. For NR, the *ARFCN-ValueNR* corresponds to a GSCN value as specified in TS 38.101 [85]. |
| ***carrierFreqs***The list of GERAN carrier frequencies organised into one group of GERAN carrier frequencies. |
| ***cellInfoList***Used to provide system information of one or more cells on the redirected inter-RAT carrier frequency. The system information can be used if, upon redirection, the UE selects an inter-RAT cell indicated by the *physCellId* and *carrierFreq* (GERAN and UTRA TDD) or by the *physCellId* (other RATs). The choice shall match the *redirectedCarrierInfo*. In particular, E-UTRAN only applies value *utra-TDD-r10* in case *redirectedCarrierInfo* is set to *utra-TDD-r10*. |
| ***cellList***Indicates a list of cells configured as RAN area. For each element, in the absence of *plmn-Identity* the UE considers the registered PLMN. Total number of cells across all PLMNs does not exceed 32. |
| ***cn-Type***The*cn-Type* is used to indicate that the UE is redirected from 5GC to EPC or 5GC when*redirectedCarrierInfo* indicates E-UTRA frequency. |
| ***drb-ContinueROHC***This field indicates whether to continue or reset the header compression protocol context for the DRBs configured with the header compression protocol. Presence of the field indicates that the header compression protocol context continues when UE initiates UP-EDT in the same cell, while absence indicates that the header compression protocol context is reset.  |
| ***dummy***This field is not used in the specification. If received it shall be ignored by the UE. |
| ***extendedWaitTime***Value in seconds for the wait time for Delay Tolerant access requests. |
| ***freqPriorityListX***Provides a cell reselection priority for each frequency, by means of separate lists for each RAT (including E-UTRA). The UE shall be able to store at least 3 occurrences of *FreqsPriorityGERAN*. If E-UTRAN includes *freqPriorityListEUTRA-v9e0* and/or *freqPriorityListEUTRA-v1310* it includes the same number of entries, and listed in the same order, as in *freqPriorityListEUTRA* (i.e. without suffix). Field *freqPriorityListExt* includes additional neighbouring inter-frequencies, i.e. extending the size of the inter-frequency carrier list using the general principles specified in 5.1.2. EUTRAN only includes *freqPriorityListExtEUTRA* if *freqPriorityListEUTRA* (i.e without suffix) includes *maxFreq* entries. If E-UTRAN includes *freqPriorityListExtEUTRA-v1310* it includes the same number of entries, and listed in the same order, as in *freqPriorityListExtEUTRA-r12.* |
| ***idleModeMobilityControlInfo***Provides dedicated cell reselection priorities. Used for cell reselection as specified in TS 36.304 [4]. For E-UTRA and UTRA frequencies, a UE that supports multi-band cells for the concerned RAT considers the dedicated priorities to be common for all overlapping bands (i.e. regardless of the ARFCN that is used). |
| ***measIdleConfig***Indicates a one-shot measurement configuration to be stored and used by the UE while in RRC\_IDLE or RRC\_INACTIVE. |
| ***mpsPriorityIndication***Indicates the UE can set the establishment cause to *highPriorityAccess* for a new connection following a redirect to E-UTRA or set the resume cause to *highPriorityAccess* for a resume following a redirect to E-UTRA. If the target RAT is NR, see TS 38.331 [82]. The eNB/ng-eNB sets the indication only for UEs authorized to receive MPS treatment as indicated by ARP and/or QoS characteristics at the eNB/ng-eNB, and it is applicable only for this instance of release with redirection to carrier/RAT included in the *redirectedCarrierInfo* field in the *RRCConnectionRelease* message. |
| ***noLastCellUpdate***Presence of the field indicates that the last used cell for (G)WUS shall not be updated. |
| ***periodic-RNAU-timer***Refers to the timer that triggers the periodic RNAU procedure in UE. Value min5 corresponds to 5 minutes, value min10 corresponds to 10 minutes and so on. |
| ***ran-Area***Indicates whether TA code(s) or RAN area code(s) are used for the RAN notification area. The network uses only TA code(s) or RAN area code(s) to configure a UE. Total number of TACs across all PLMNs does not exceed 16. Total number of RAN-AreaCode across all PLMNs does not exceed 32. |
| ***ran-NotificationAreaInfo***Network ensures that the UE in RRC\_INACTIVE always has a valid *ran-NotificationAreaInfo*. |
| ***ranAreaConfigList***Indicates a list of RAN area codes or RA code(s) as RAN area. For each element, in the absence of *plmn-Identity* the UE considers the registered PLMN. |
| ***ran-pagingCycle***Refers to the UE specific cycle for RAN-initiated paging. Value rf32 corresponds to 32 radio frames, rf64 corresponds to 64 radio frames and so on. |
| ***redirectedCarrierInfo***The r*edirectedCarrierInfo* indicates a carrier frequency (downlink for FDD) and is used to redirect the UE to an E‑UTRA or an inter-RAT carrier frequency, by means of the cell selection upon leaving RRC\_CONNECTED as specified in TS 36.304 [4]. The value *geran* can only be included after successful security activation when UE is connected to 5GC. |
| ***releaseCause***The *releaseCause* is used to indicate the reason for releasing the RRC Connection. The cause value *cs-FallbackHighPriority* is only applicable when *redirectedCarrierInfo* is present with the value set to *utra-FDD,* *utra-TDD* or *utra-TDD-r10*. E-UTRAN should not set the *releaseCause* to *loadBalancingTAURequired* or to *cs-FallbackHighPriority* if the *extendedWaitTime* is present. The network should not set the *releaseCause* to *loadBalancingTAURequired* if the UE is connected to 5GC. The network does not set the *releaseCause* to *rrc-Suspend* if the UE is configured with a DAPS bearer, i.e. if source PCell resources after a DAPS handover have not been released. |
| ***releaseIdleMeasConfig***Indicates that the UE shall release the idle/inactive measurement configurations, if configured. |
| ***rrc-InactiveConfig***Indicates configuration for the RRC\_INACTIVE state. The network does not configure this field when the UE is redirected to an inter-RAT carrier frequency or if the UE is configured with a DAPS bearer. |
| ***satAssistanceInfoList***List of satellite ID(s), used to associate with the satellite assistance information for neighbour cell measurements on this frequency for the purpose of redirection. Each satellite ID included in this list corresponds to a *satelliteId* configured in *neighSatelliteInfoListNR* via *SystemInformationBlockType33.* |
| ***smtc***The SSB periodicity/offset/duration configuration of the redirected target NR frequency. It is based on the timing reference of EUTRAN PCell. If the field is absent, the UE uses the SMTC configured in the *measObjectNR* having the same SSB frequency and subcarrier spacing |
| ***subcarrierSpacingSSB***Indicate subcarrier spacing of SSB of redirected target NR frequency. Only the values 15 kHz or 30 kHz (FR1), 120 kHz or 240 kHz (FR2-1), 120kHz or 480kHz (FR2-2) are applicable. |
| ***systemInformation***Container for system information of the GERAN cell i.e. one or more System Information (SI) messages as defined in TS 44.018 [45], table 9.1.1.  |
| ***t320***Timer T320 as described in clause 7.3. Value minN corresponds to N minutes. |
| ***t323***Timer T323 as described in clause 7.3. Value minN corresponds to N minutes. |
| ***utra-BCCH-Container***Contains System Information Container message as defined in TS 25.331 [19]. |
| ***waitTime***Wait time value in seconds. |

| Conditional presence | Explanation |
| --- | --- |
| *5GC* | The field is optionally present, Need ON, if the UE is connected to 5GC; otherwise the field is not present. |
| *BLCE-IDLEeDRX* | The field is optionally present, Need OR, if the UE is a BL UE or UE in CE and the UE is connected to 5GC and IDLE mode eDRX is configured and *ran-PagingCycle-r15* is absent; otherwise the field is not present. |
| *EARFCN-max* | The field is mandatory present if the corresponding *carrierFreq* (i.e. without suffix) is set to *maxEARFCN*. Otherwise the field is not present. |
| *EarlySec* | When the UE is connected to 5GC, the field is mandatory present. When the UE is connected to EPC, the field is optionally present, Need ON, if the UE supports UP-EDT or UP transmission using PUR or early security reactivation and *releaseCause* is set to *rrc-Suspend*; otherwise the field is not present. |
| *IdleInfoEUTRA* | The field is optionally present, Need OP, if the *IdleModeMobilityControlInfo* (i.e. without suffix) is included and includes *freqPriorityListEUTRA*; otherwise the field is not present. |
| *INACTIVE* | The field is mandatory present in this release. |
| *NoRedirect-r8* | The field is optionally present, Need OP, if the *redirectedCarrierInfo* (i.e. without suffix) is not included; otherwise the field is not present. |
| *Redirection* | The field is optionally present, Need ON, if the *redirectedCarrierInfo* is included and set to *geran*, *utra-FDD*, *utra-TDD* or *utra-TDD-r10*; otherwise the field is not present. |
| *Redirection2* | The field is optionally present, Need OR, if *redirectedCarrierInfo* is included; otherwise the field is not present. |
| *UP-EDTorPUR* | The field is optionally present, Need ON, if the UE supports UP-EDT or UP transmission using PUR and *releaseCause* is set to *rrc-Suspend*; otherwise the field is not present. |

<Irrelevant Texts Omitted>

|  |
| --- |
| Next change |

### 6.3.1 System information blocks

<Irrelevant Texts Omitted>

#### – *SystemInformationBlockType3*

The IE *SystemInformationBlockType3* contains cell re-selection information common for intra-frequency, inter-frequency and/ or inter-RAT cell re-selection (i.e. applicable for more than one type of cell re-selection but not necessarily all) as well as intra-frequency cell re-selection information other than neighbouring cell related.

*SystemInformationBlockType3* information element

-- ASN1START

SystemInformationBlockType3 ::= SEQUENCE {

 cellReselectionInfoCommon SEQUENCE {

 q-Hyst ENUMERATED {

 dB0, dB1, dB2, dB3, dB4, dB5, dB6, dB8, dB10,

 dB12, dB14, dB16, dB18, dB20, dB22, dB24},

 speedStateReselectionPars SEQUENCE {

 mobilityStateParameters MobilityStateParameters,

 q-HystSF SEQUENCE {

 sf-Medium ENUMERATED {

 dB-6, dB-4, dB-2, dB0},

 sf-High ENUMERATED {

 dB-6, dB-4, dB-2, dB0}

 }

 } OPTIONAL -- Need OP

 },

 cellReselectionServingFreqInfo SEQUENCE {

 s-NonIntraSearch ReselectionThreshold OPTIONAL, -- Need OP

 threshServingLow ReselectionThreshold,

 cellReselectionPriority CellReselectionPriority

 },

 intraFreqCellReselectionInfo SEQUENCE {

 q-RxLevMin Q-RxLevMin,

 p-Max P-Max OPTIONAL, -- Need OP

 s-IntraSearch ReselectionThreshold OPTIONAL, -- Need OP

 allowedMeasBandwidth AllowedMeasBandwidth OPTIONAL, -- Need OP

 presenceAntennaPort1 PresenceAntennaPort1,

 neighCellConfig NeighCellConfig,

 t-ReselectionEUTRA T-Reselection,

 t-ReselectionEUTRA-SF SpeedStateScaleFactors OPTIONAL -- Need OP

 },

 ...,

 lateNonCriticalExtension OCTET STRING (CONTAINING SystemInformationBlockType3-v10j0-IEs) OPTIONAL,

 [[ s-IntraSearch-v920 SEQUENCE {

 s-IntraSearchP-r9 ReselectionThreshold,

 s-IntraSearchQ-r9 ReselectionThresholdQ-r9

 } OPTIONAL, -- Need OP

 s-NonIntraSearch-v920 SEQUENCE {

 s-NonIntraSearchP-r9 ReselectionThreshold,

 s-NonIntraSearchQ-r9 ReselectionThresholdQ-r9

 } OPTIONAL, -- Need OP

 q-QualMin-r9 Q-QualMin-r9 OPTIONAL, -- Need OP

 threshServingLowQ-r9 ReselectionThresholdQ-r9 OPTIONAL -- Need OP

 ]],

 [[ q-QualMinWB-r11 Q-QualMin-r9 OPTIONAL -- Cond WB-RSRQ

 ]],

 [[ q-QualMinRSRQ-OnAllSymbols-r12 Q-QualMin-r9 OPTIONAL -- Cond RSRQ

 ]],

 [[ cellReselectionServingFreqInfo-v1310 CellReselectionServingFreqInfo-v1310 OPTIONAL, -- Need OP

 redistributionServingInfo-r13 RedistributionServingInfo-r13 OPTIONAL, --Need OR

 cellSelectionInfoCE-r13 CellSelectionInfoCE-r13 OPTIONAL, -- Need OP

 t-ReselectionEUTRA-CE-r13 T-ReselectionEUTRA-CE-r13 OPTIONAL-- Need OP

 ]],

 [[ cellSelectionInfoCE1-r13 CellSelectionInfoCE1-r13 OPTIONAL -- Need OP

 ]],

 [[ cellSelectionInfoCE1-v1360 CellSelectionInfoCE1-v1360 OPTIONAL -- Cond QrxlevminCE1

 ]],

 [[ cellReselectionInfoCommon-v1460 CellReselectionInfoCommon-v1460 OPTIONAL -- Need OR

 ]],

 [[ cellReselectionInfoHSDN-r15 CellReselectionInfoHSDN-r15 OPTIONAL, -- Need OR

 cellSelectionInfoCE-v1530 CellSelectionInfoCE-v1530 OPTIONAL, -- Need OP

 crs-IntfMitigNeighCellsCE-r15 ENUMERATED {enabled} OPTIONAL -- Need OP

 ]],

 [[ cellReselectionServingFreqInfo-v1610 CellReselectionServingFreqInfo-v1610 OPTIONAL -- Need OR

 ]],

 [[ t-Service-r17 TimeOffsetUTC-r17 OPTIONAL -- Need OR

 ]],

 [[ satelliteAssistanceInfoList-r18

 SEQUENCE (SIZE(1..maxSat-r17)) OF SatelliteId-r18 OPTIONAL, -- Need OR

 freqBandInfoAerial-r18 NS-PmaxListAerial-r18 OPTIONAL, -- Need OR

 multiBandInfoListAerial-r18 MultiBandInfoListAerial-r18 OPTIONAL -- Need OR

 ]]

}

RedistributionServingInfo-r13 ::= SEQUENCE {

 redistributionFactorServing-r13 INTEGER(0..10),

 redistributionFactorCell-r13 ENUMERATED{true} OPTIONAL, --Need OP

 t360-r13 ENUMERATED {min4, min8, min16, min32,infinity,

 spare3,spare2,spare1},

 redistrOnPagingOnly-r13 ENUMERATED {true} OPTIONAL --Need OP

}

CellReselectionServingFreqInfo-v1310 ::= SEQUENCE {

 cellReselectionSubPriority-r13 CellReselectionSubPriority-r13

}

CellReselectionServingFreqInfo-v1610 ::= SEQUENCE {

 altCellReselectionPriority-r16 CellReselectionPriority OPTIONAL, -- Need OR

 altCellReselectionSubPriority-r16 CellReselectionSubPriority-r13 OPTIONAL -- Need OR

}

-- Late non critical extensions

SystemInformationBlockType3-v10j0-IEs ::= SEQUENCE {

 freqBandInfo-r10 NS-PmaxList-r10 OPTIONAL, -- Need OR

 multiBandInfoList-v10j0 MultiBandInfoList-v10j0 OPTIONAL, -- Need OR

 nonCriticalExtension SystemInformationBlockType3-v10l0-IEs OPTIONAL

}

SystemInformationBlockType3-v10l0-IEs ::= SEQUENCE {

 freqBandInfo-v10l0 NS-PmaxList-v10l0 OPTIONAL, -- Need OR

 multiBandInfoList-v10l0 MultiBandInfoList-v10l0 OPTIONAL, -- Need OR

 nonCriticalExtension SEQUENCE {} OPTIONAL

}

CellReselectionInfoCommon-v1460 ::= SEQUENCE {

 s-SearchDeltaP-r14 ENUMERATED {dB6, dB9, dB12, dB15}

}

CellReselectionInfoHSDN-r15 ::= SEQUENCE {

 cellEquivalentSize-r15 INTEGER(2..16)

}

-- ASN1STOP

| *SystemInformationBlockType3* field descriptions |
| --- |
| ***allowedMeasBandwidth***If absent, the value corresponding to the downlink bandwidth indicated by the *dl-Bandwidth* included in *MasterInformationBlock* applies. |
| ***altCellReselectionPriority***Alternative cell reselection priorities to be used by the UEs for which the *altFreqPriorities* is set to *true* in the *RRCConnectionRelease* message. |
| ***altCellReselectionSubPriority***Alternative cell reselection sub-priorities to be used by the UEs for which the *altFreqPriorities* is set to *true* in the *RRCConnectionRelease* message. |
| ***cellEquivalentSize***The number of cell count used for mobility state estimation for this cell as specified in TS 36.304 [4].  |
| ***cellSelectionInfoCE***Parameters included in coverage enhancement S criteria for BL UEs and UEs in CE, applicable for intra-frequency neighbour cells. If absent, coverage enhancement S criteria is not applicable. |
| ***cellSelectionInfoCE1***Parameters included in coverage enhancement S criteria for BL UEs and UEs in CE supporting CE Mode B, applicable for intra-frequency neighbour cells. E-UTRAN includes this IE only if *cellSelectionInfoCE* in SIB3 is present. |
| ***cellReselectionInfoCommon***Cell re-selection information common for cells. |
| ***cellReselectionServingFreqInfo***Information common for Cell re-selection to inter-frequency and inter-RAT cells. |
| ***crs-IntfMitigNeighCellsCE***For BL UEs supporting *ce-CRS-IntfMitig*, this field indicates CRS interference mitigation, as specified in TS 36.133 [16], clause 3.6.1.2 and 3.6.1.3, is enabled in any of the intra-frequency neibhour cells, and the UE shall perform intra-frequency neighbour cell RRM measurements in the center 6 PRBs. |
| ***freqBandInfo***A list of *additionalPmax* and *additionalSpectrumEmission* values, as defined in TS 36.101 [42], table 6.2.4-1, for UEs neither in CE nor BL UEs, TS 36.101 [42], table 6.2.4E-1, for UEs in CE or BL UEs and TS 36.102 [113], table 6.2A.3-1, for NTN capable UE, applicable for the intra-frequency neighouring E-UTRA cells if the UE selects the frequency band from *freqBandIndicator* in *SystemInformationBlockType1*. If E-UTRAN includes *freqBandInfo-v10l0* it includes the same number of entries, and listed in the same order, as in *freqBandInfo-r10*. |
| ***intraFreqcellReselectionInfo***Cell re-selection information common for intra-frequency cells. |
| ***multiBandInfoList-v10j0***A list of *additionalPmax* and *additionalSpectrumEmission* values, as defined in TS 36.101 [42], table 6.2.4-1, for UEs neither in CE nor BL UEs, TS 36.101 [42], table 6.2.4E-1, for UEs in CE or BL UEs and TS 36.102 [113], table 6.2A.3-1, for NTN capable UE, applicable for the intra-frequency neighouring E-UTRA cells if the UE selects the frequency bands in *multiBandInfoList* (i.e. without suffix) or *multiBandInfoList-v9e0* in *SystemInformationBlockType1*. If E-UTRAN includes *multiBandInfoList-v10j0*, it includes the same number of entries, and listed in the same order, as in *multiBandInfoList* (i.e. without suffix) in *SystemInformationBlockType1*. If E-UTRAN includes *multiBandInfoList-v10l0* it includes the same number of entries, and listed in the same order, as in *multiBandInfoList-v10j0*. |
| ***p-Max***Value applicable for the intra-frequency neighbouring E-UTRA cells. If absent the UE applies the maximum power according to its capability as specified in TS 36.101 [42], clause 6.2.2. This field is ignored by IAB-MT. The IAB-MT applies output power and emissions requirements, as specified in TS 38.174 [107]. |
| ***redistrOnPagingOnly***If this field is present and the UE is redistribution capable, the UE shall only wait for the paging message to trigger E-UTRAN inter-frequency redistribution procedure as specified in clause 5.2.4.10 of TS 36.304 [4]. |
| ***q-Hyst***Parameter *Qhyst* in TS 36.304 [4], Value in dB. Value dB1 corresponds to 1 dB, dB2 corresponds to 2 dB and so on. |
| ***q-HystSF***Parameter "Speed dependent ScalingFactor for *Qhyst*" in TS 36.304 [4]. The sf-Medium and sf-High concern the additional hysteresis to be applied, in Medium and High Mobility state respectively, to *Qhyst* as defined in TS 36.304 [4]. In dB. Value dB-6 corresponds to -6dB, dB-4 corresponds to -4dB and so on. |
| ***q-QualMin***Parameter "Qqualmin" in TS 36.304 [4], applicable for intra-frequency neighbour cells. If the field is not present, the UE applies the (default) value of negative infinity for Qqualmin. NOTE 1. |
| ***q-QualMinRSRQ-OnAllSymbols***If this field is present and supported by the UE, the UE shall, when performing RSRQ measurements, perform RSRQ measurement on all OFDM symbols in accordance with TS 36.214 [48]. NOTE 1. |
| ***q-QualMinWB***If this field is present and supported by the UE, the UE shall, when performing RSRQ measurements, use a wider bandwidth in accordance with TS 36.133 [16]. NOTE 1. |
| ***q-RxLevMin***Parameter "Qrxlevmin" in TS 36.304 [4], applicable for intra-frequency neighbour cells. |
| ***redistributionFactorCell***If *redistributionFactorCell* is present, *redistributionFactorServing* is only applicable for the serving cell otherwise it is applicable for serving frequency |
| ***redistributionFactorServing***Parameter *redistributionFactorServing* in TS 36.304 [4]. |
| ***s-IntraSearch***Parameter "SIntraSearchP" in TS 36.304 [4]. If the field *s-IntraSearchP* is present, the UE applies the value of *s-IntraSearchP* instead. Otherwise if neither *s-IntraSearch* nor *s-IntraSearchP* is present, the UE applies the (default) value of infinity for SIntraSearchP. |
| ***s-IntraSearchP***Parameter "SIntraSearchP" in TS 36.304 [4]. See descriptions under *s-IntraSearch*. |
| ***s-IntraSearchQ***Parameter "SIntraSearchQ" in TS 36.304 [4]. If the field is not present, the UE applies the (default) value of 0 dB for SIntraSearchQ. |
| ***s-NonIntraSearch***Parameter "SnonIntraSearchP" in TS 36.304 [4]. If the field *s-NonIntraSearchP* is present, the UE applies the value of *s-NonIntraSearchP* instead. Otherwise if neither *s-NonIntraSearch* nor *s-NonIntraSearchP* is present, the UE applies the (default) value of infinity for SnonIntraSearchP. |
| ***s-NonIntraSearchP***Parameter "SnonIntraSearchP" in TS 36.304 [4]. See descriptions under *s-NonIntraSearch*. |
| ***s-NonIntraSearchQ***Parameter "SnonIntraSearchQ" in TS 36.304 [4]. If the field is not present, the UE applies the (default) value of 0 dB for SnonIntraSearchQ. |
| ***s-SearchDeltaP***Parameter "SSearchDeltaP" in TS 36.304 [4]. This parameter is only applicable for UEs supporting relaxed monitoring as specified in TS 36.306 [5]. Value dB6 corresponds to 6 dB, dB9 corresponds to 9 dB and so on. |
| ***satelliteAssistanceInfoList***List of satellite ID(s), used to associate with the satellite assistance information in *SystemInformationBlockType31* and *SystemInformationBlockType33* for intra-frequency neighbour cell measurements. Each satellite ID included in this list corresponds to a *satelliteId* configured via *SystemInformationBlockType31* or in *neighSatelliteInfoList* via *SystemInformationBlockType33.* |
| ***speedStateReselectionPars***Speed dependent reselection parameters, see TS 36.304 [4]. If this field is absent, i.e, *mobilityStateParameters* is also not present, UE behaviour is specified in TS 36.304 [4]. |
| ***t-Service***Time information on when an NTN cell is going to stop serving the area it is currently covering, as specified in TS 36.304 [4]. This field applies for service link switches in NTN quasi-Earth fixed cells and feeder link switches for both NTN quasi-Earth fixed and earth-moving cells. |
| ***t360***Parameter "T360" in TS 36.304 [4]. Value *min4* corresponds to 4 minutes, value *min8* corresponds to 8 minutes, and so on. |
| ***threshServingLow***Parameter "ThreshServing, LowP" in TS 36.304 [4]. |
| ***threshServingLowQ***Parameter "ThreshServing, LowQ" in TS 36.304 [4]. |
| ***t-ReselectionEUTRA***Parameter "TreselectionEUTRA" in TS 36.304 [4]. |
| ***t-ReselectionEUTRA-SF***Parameter "Speed dependent ScalingFactor for TreselectionEUTRA" in TS 36.304 [4]. If the field is not present, the UE behaviour is specified in TS 36.304 [4]. |

NOTE 1: The value the UE applies for parameter "Qqualmin" in TS 36.304 [4] depends on the *q-QualMin* fields signalled by E-UTRAN and supported by the UE. In case multiple candidate options are available, the UE shall select the highest priority candidate option according to the priority order indicated by the following table (top row is highest priority).

|  |  |  |
| --- | --- | --- |
| q-QualMinRSRQ-OnAllSymbols | q-QualMinWB | Value of parameter "Qqualmin" in TS 36.304 [4] |
| Included | Included | *q-QualMinRSRQ-OnAllSymbols* – (*q-QualMin* – *q-QualMinWB*) |
| Included | Not included | *q-QualMinRSRQ-OnAllSymbols* |
| Not included | Included | *q-QualMinWB* |
| Not included | Not included | *q-QualMin* |

| Conditional presence | Explanation |
| --- | --- |
| *QrxlevminCE1* | The field is optionally present, Need OR, if *q-RxLevMinCE1-r13* is set below -140 dBm. Otherwise the field is not present. |
| *RSRQ* | The field is optionally present, Need OR, if *threshServingLowQ* is present in SIB3; otherwise it is not present. |
| *WB-RSRQ* | The field is optionally present, need OP if the measurement bandwidth indicated by *allowedMeasBandwidth* is 50 resource blocks or larger; otherwise it is not present. |

<Irrelevant Texts Omitted>

#### – *SystemInformationBlockType5*

The IE *SystemInformationBlockType5* contains information relevant for inter-frequency cell re-selection (i.e. information about other E‑UTRA frequencies and inter-frequency neighbouring cells relevant for cell re-selection) and information relevant for E-UTRA and NR idle/inactive measurements. The IE includes cell re-selection parameters common for a frequency as well as cell specific re-selection parameters.

*SystemInformationBlockType5* information element

-- ASN1START

SystemInformationBlockType5 ::= SEQUENCE {

 interFreqCarrierFreqList InterFreqCarrierFreqList,

 ...,

 lateNonCriticalExtension OCTET STRING (CONTAINING SystemInformationBlockType5-v8h0-IEs) OPTIONAL,

 [[ interFreqCarrierFreqList-v1250 InterFreqCarrierFreqList-v1250 OPTIONAL, -- Need OR

 interFreqCarrierFreqListExt-r12 InterFreqCarrierFreqListExt-r12 OPTIONAL -- Need OR

 ]],

 [[ interFreqCarrierFreqListExt-v1280 InterFreqCarrierFreqListExt-v1280 OPTIONAL -- Need OR

 ]],

 [[ interFreqCarrierFreqList-v1310 InterFreqCarrierFreqList-v1310 OPTIONAL, -- Need OR

 interFreqCarrierFreqListExt-v1310 InterFreqCarrierFreqListExt-v1310 OPTIONAL -- Need OR

 ]],

 [[ interFreqCarrierFreqList-v1350 InterFreqCarrierFreqList-v1350 OPTIONAL, -- Need OR

 interFreqCarrierFreqListExt-v1350 InterFreqCarrierFreqListExt-v1350 OPTIONAL -- Need OR

 ]],

 [[ interFreqCarrierFreqListExt-v1360 InterFreqCarrierFreqListExt-v1360 OPTIONAL -- Need OR

 ]],

 [[ scptm-FreqOffset-r14 INTEGER (1..8) OPTIONAL -- Need OP

 ]],

 [[ interFreqCarrierFreqList-v1530 InterFreqCarrierFreqList-v1530 OPTIONAL, -- Need OR

 interFreqCarrierFreqListExt-v1530 InterFreqCarrierFreqListExt-v1530 OPTIONAL, -- Need OR

 measIdleConfigSIB-r15 MeasIdleConfigSIB-r15 OPTIONAL -- Need OR

 ]],

 [[ interFreqCarrierFreqList-v1610 InterFreqCarrierFreqList-v1610 OPTIONAL, -- Need OR

 interFreqCarrierFreqListExt-v1610 InterFreqCarrierFreqListExt-v1610 OPTIONAL, -- Need OR

 measIdleConfigSIB-NR-r16 MeasIdleConfigSIB-NR-r16 OPTIONAL -- Need OR

 ]],

 [[ interFreqCarrierFreqList-v1800 InterFreqCarrierFreqList-v1800 OPTIONAL, -- Need OR

 interFreqCarrierFreqListExt-v1800 InterFreqCarrierFreqListExt-v1800 OPTIONAL -- Need OR

 ]]

}

-- Late non critical extensions

SystemInformationBlockType5-v8h0-IEs ::= SEQUENCE {

 interFreqCarrierFreqList-v8h0 SEQUENCE (SIZE (1..maxFreq)) OF InterFreqCarrierFreqInfo-v8h0 OPTIONAL, -- Need OP

 nonCriticalExtension SystemInformationBlockType5-v9e0-IEs OPTIONAL

}

SystemInformationBlockType5-v9e0-IEs ::= SEQUENCE {

 interFreqCarrierFreqList-v9e0 SEQUENCE (SIZE (1..maxFreq)) OF InterFreqCarrierFreqInfo-v9e0 OPTIONAL, -- Need OR

 nonCriticalExtension SystemInformationBlockType5-v10j0-IEs OPTIONAL

}

SystemInformationBlockType5-v10j0-IEs ::= SEQUENCE {

 interFreqCarrierFreqList-v10j0 SEQUENCE (SIZE (1..maxFreq)) OF InterFreqCarrierFreqInfo-v10j0 OPTIONAL, -- Need OR

 nonCriticalExtension SystemInformationBlockType5-v10l0-IEs OPTIONAL

}

SystemInformationBlockType5-v10l0-IEs ::= SEQUENCE {

 interFreqCarrierFreqList-v10l0 SEQUENCE (SIZE (1..maxFreq)) OF InterFreqCarrierFreqInfo-v10l0 OPTIONAL, -- Need OR

 nonCriticalExtension SystemInformationBlockType5-v13a0-IEs OPTIONAL

}

SystemInformationBlockType5-v13a0-IEs ::= SEQUENCE {

 -- Late non critical extensions from REL-10 upto REL-12

 lateNonCriticalExtension OCTET STRING OPTIONAL, -- Need OR

 interFreqCarrierFreqList-v13a0 InterFreqCarrierFreqList-v13a0 OPTIONAL, -- Need OR

 -- Late non critical extensions from REL-13

 nonCriticalExtension SEQUENCE {} OPTIONAL

}

InterFreqCarrierFreqList ::= SEQUENCE (SIZE (1..maxFreq)) OF InterFreqCarrierFreqInfo

InterFreqCarrierFreqList-v1250 ::= SEQUENCE (SIZE (1..maxFreq)) OF InterFreqCarrierFreqInfo-v1250

InterFreqCarrierFreqList-v1310 ::= SEQUENCE (SIZE (1..maxFreq)) OF InterFreqCarrierFreqInfo-v1310

InterFreqCarrierFreqList-v1350 ::= SEQUENCE (SIZE (1..maxFreq)) OF InterFreqCarrierFreqInfo-v1350

InterFreqCarrierFreqList-v13a0 ::= SEQUENCE (SIZE (1..maxFreq)) OF InterFreqCarrierFreqInfo-v1360

InterFreqCarrierFreqList-v1530 ::= SEQUENCE (SIZE (1..maxFreq)) OF InterFreqCarrierFreqInfo-v1530

InterFreqCarrierFreqList-v1610 ::= SEQUENCE (SIZE (1..maxFreq)) OF InterFreqCarrierFreqInfo-v1610

InterFreqCarrierFreqList-v1800 ::= SEQUENCE (SIZE (1..maxFreq)) OF InterFreqCarrierFreqInfo-v1800

InterFreqCarrierFreqListExt-r12 ::= SEQUENCE (SIZE (1..maxFreq)) OF InterFreqCarrierFreqInfo-r12

InterFreqCarrierFreqListExt-v1280 ::= SEQUENCE (SIZE (1..maxFreq)) OF InterFreqCarrierFreqInfo-v10j0

InterFreqCarrierFreqListExt-v1310 ::= SEQUENCE (SIZE (1..maxFreq)) OF InterFreqCarrierFreqInfo-v1310

InterFreqCarrierFreqListExt-v1350 ::= SEQUENCE (SIZE (1..maxFreq)) OF InterFreqCarrierFreqInfo-v1350

InterFreqCarrierFreqListExt-v1360 ::= SEQUENCE (SIZE (1..maxFreq)) OF InterFreqCarrierFreqInfo-v1360

InterFreqCarrierFreqListExt-v1530 ::= SEQUENCE (SIZE (1..maxFreq)) OF InterFreqCarrierFreqInfo-v1530

InterFreqCarrierFreqListExt-v1610 ::= SEQUENCE (SIZE (1..maxFreq)) OF InterFreqCarrierFreqInfo-v1610

InterFreqCarrierFreqListExt-v1800 ::= SEQUENCE (SIZE (1..maxFreq)) OF InterFreqCarrierFreqInfo-v1800

InterFreqCarrierFreqInfo ::= SEQUENCE {

 dl-CarrierFreq ARFCN-ValueEUTRA,

 q-RxLevMin Q-RxLevMin,

 p-Max P-Max OPTIONAL, -- Need OP

 t-ReselectionEUTRA T-Reselection,

 t-ReselectionEUTRA-SF SpeedStateScaleFactors OPTIONAL, -- Need OP

 threshX-High ReselectionThreshold,

 threshX-Low ReselectionThreshold,

 allowedMeasBandwidth AllowedMeasBandwidth,

 presenceAntennaPort1 PresenceAntennaPort1,

 cellReselectionPriority CellReselectionPriority OPTIONAL, -- Need OP

 neighCellConfig NeighCellConfig,

 q-OffsetFreq Q-OffsetRange DEFAULT dB0,

 interFreqNeighCellList InterFreqNeighCellList OPTIONAL, -- Need OR

 interFreqExcludedCellList InterFreqExcludedCellList OPTIONAL, -- Need OR

 ...,

 [[ q-QualMin-r9 Q-QualMin-r9 OPTIONAL, -- Need OP

 threshX-Q-r9 SEQUENCE {

 threshX-HighQ-r9 ReselectionThresholdQ-r9,

 threshX-LowQ-r9 ReselectionThresholdQ-r9

 } OPTIONAL -- Cond RSRQ

 ]],

 [[ q-QualMinWB-r11 Q-QualMin-r9 OPTIONAL -- Cond WB-RSRQ

 ]]

}

InterFreqCarrierFreqInfo-v8h0 ::= SEQUENCE {

 multiBandInfoList MultiBandInfoList OPTIONAL -- Need OR

}

InterFreqCarrierFreqInfo-v9e0 ::= SEQUENCE {

 dl-CarrierFreq-v9e0 ARFCN-ValueEUTRA-v9e0 OPTIONAL, -- Cond dl-FreqMax

 multiBandInfoList-v9e0 MultiBandInfoList-v9e0 OPTIONAL -- Need OR

}

InterFreqCarrierFreqInfo-v10j0 ::= SEQUENCE {

 freqBandInfo-r10 NS-PmaxList-r10 OPTIONAL, -- Need OR

 multiBandInfoList-v10j0 MultiBandInfoList-v10j0 OPTIONAL -- Need OR

}

InterFreqCarrierFreqInfo-v10l0 ::= SEQUENCE {

 freqBandInfo-v10l0 NS-PmaxList-v10l0 OPTIONAL, -- Need OR

 multiBandInfoList-v10l0 MultiBandInfoList-v10l0 OPTIONAL -- Need OR

}

InterFreqCarrierFreqInfo-v1250 ::= SEQUENCE {

 reducedMeasPerformance-r12 ENUMERATED {true} OPTIONAL, -- Need OP

 q-QualMinRSRQ-OnAllSymbols-r12 Q-QualMin-r9 OPTIONAL -- Cond RSRQ2

}

InterFreqCarrierFreqInfo-r12 ::= SEQUENCE {

 dl-CarrierFreq-r12 ARFCN-ValueEUTRA-r9,

 q-RxLevMin-r12 Q-RxLevMin,

 p-Max-r12 P-Max OPTIONAL, -- Need OP

 t-ReselectionEUTRA-r12 T-Reselection,

 t-ReselectionEUTRA-SF-r12 SpeedStateScaleFactors OPTIONAL, -- Need OP

 threshX-High-r12 ReselectionThreshold,

 threshX-Low-r12 ReselectionThreshold,

 allowedMeasBandwidth-r12 AllowedMeasBandwidth,

 presenceAntennaPort1-r12 PresenceAntennaPort1,

 cellReselectionPriority-r12 CellReselectionPriority OPTIONAL, -- Need OP

 neighCellConfig-r12 NeighCellConfig,

 q-OffsetFreq-r12 Q-OffsetRange DEFAULT dB0,

 interFreqNeighCellList-r12 InterFreqNeighCellList OPTIONAL, -- Need OR

 interFreqExcludedCellList-r12 InterFreqExcludedCellList OPTIONAL, -- Need OR

 q-QualMin-r12 Q-QualMin-r9 OPTIONAL, -- Need OP

 threshX-Q-r12 SEQUENCE {

 threshX-HighQ-r12 ReselectionThresholdQ-r9,

 threshX-LowQ-r12 ReselectionThresholdQ-r9

 } OPTIONAL, -- Cond RSRQ

 q-QualMinWB-r12 Q-QualMin-r9 OPTIONAL, -- Cond WB-RSRQ

 multiBandInfoList-r12 MultiBandInfoList-r11 OPTIONAL, -- Need OR

 reducedMeasPerformance-r12 ENUMERATED {true} OPTIONAL, -- Need OP

 q-QualMinRSRQ-OnAllSymbols-r12 Q-QualMin-r9 OPTIONAL, -- Cond RSRQ2

...

}

InterFreqCarrierFreqInfo-v1310 ::= SEQUENCE {

 cellReselectionSubPriority-r13 CellReselectionSubPriority-r13 OPTIONAL, -- Need OP

 redistributionInterFreqInfo-r13 RedistributionInterFreqInfo-r13 OPTIONAL, --Need OP

 cellSelectionInfoCE-r13 CellSelectionInfoCE-r13 OPTIONAL, -- Need OP

 t-ReselectionEUTRA-CE-r13 T-ReselectionEUTRA-CE-r13 OPTIONAL -- Need OP

}

InterFreqCarrierFreqInfo-v1350 ::= SEQUENCE {

 cellSelectionInfoCE1-r13 CellSelectionInfoCE1-r13 OPTIONAL -- Need OP

}

InterFreqCarrierFreqInfo-v1360 ::= SEQUENCE {

 cellSelectionInfoCE1-v1360 CellSelectionInfoCE1-v1360 OPTIONAL -- Cond QrxlevminCE1

}

InterFreqCarrierFreqInfo-v1530 ::= SEQUENCE {

 hsdn-Indication-r15 BOOLEAN,

 interFreqNeighHSDN-CellList-r15 InterFreqNeighHSDN-CellList-r15 OPTIONAL, -- Need OR

 cellSelectionInfoCE-v1530 CellSelectionInfoCE-v1530 OPTIONAL -- Need OP

}

InterFreqCarrierFreqInfo-v1610 ::= SEQUENCE {

 altCellReselectionPriority-r16 CellReselectionPriority OPTIONAL, -- Need OR

 altCellReselectionSubPriority-r16 CellReselectionSubPriority-r13 OPTIONAL, -- Need OR

 rss-ConfigCarrierInfo-r16 RSS-ConfigCarrierInfo-r16 OPTIONAL, -- Cond RSS

 interFreqNeighCellList-v1610 InterFreqNeighCellList-v1610 OPTIONAL -- Cond RSS

}

InterFreqCarrierFreqInfo-v1800 ::= SEQUENCE {

 satelliteAssistanceInfoList-r18 SEQUENCE (SIZE(1..maxSat-r17)) OF SatelliteId-r18

 OPTIONAL, -- Need OP

 freqBandIndicatorAerial-r18 FreqBandIndicator-r11 OPTIONAL, -- Need OR

 freqBandInfoAerial-r18 NS-PmaxListAerial-r18 OPTIONAL, -- Need OR

 multiBandInfoListAerial-r18 MultiBandInfoListAerial-r18 OPTIONAL -- Need OR

}

InterFreqNeighCellList ::= SEQUENCE (SIZE (1..maxCellInter)) OF InterFreqNeighCellInfo

InterFreqNeighCellList-v1610 ::= SEQUENCE (SIZE (1..maxCellInter)) OF InterFreqNeighCellInfo-v1610

InterFreqNeighHSDN-CellList-r15 ::= SEQUENCE (SIZE (1..maxCellInter)) OF PhysCellIdRange

InterFreqNeighCellInfo ::= SEQUENCE {

 physCellId PhysCellId,

 q-OffsetCell Q-OffsetRange

}

InterFreqNeighCellInfo-v1610 ::= SEQUENCE {

 rss-MeasPowerBias-r16 RSS-MeasPowerBias-r16

}

InterFreqExcludedCellList ::= SEQUENCE (SIZE (1..maxExcludedCell)) OF PhysCellIdRange

RedistributionInterFreqInfo-r13 ::= SEQUENCE {

 redistributionFactorFreq-r13 RedistributionFactor-r13 OPTIONAL, --Need OP

 redistributionNeighCellList-r13 RedistributionNeighCellList-r13 OPTIONAL --Need OP

}

RedistributionNeighCellList-r13 ::= SEQUENCE (SIZE (1..maxCellInter)) OF RedistributionNeighCell-r13

RedistributionNeighCell-r13 ::= SEQUENCE {

 physCellId-r13 PhysCellId,

 redistributionFactorCell-r13 RedistributionFactor-r13

}

RedistributionFactor-r13 ::= INTEGER(1..10)

-- ASN1STOP

| *SystemInformationBlockType5* field descriptions |
| --- |
| ***altCellReselectionPriority***Alternative cell reselection priorities to be used by the UEs for which the *altFreqPriorities* is set to *true* in the *RRCConnectionRelease* message. |
| ***altCellReselectionSubPriority***Alternative cell reselection sub-priorities to be used by the UEs for which the *altFreqPriorities* is set to *true* in the *RRCConnectionRelease* message. |
| ***cellSelectionInfoCE***Parameters included in coverage enhancement S criteria for BL UEs and UEs in CE, applicable for inter-frequency neighbour cells. If absent, coverage enhancement S criteria is not applicable. |
| ***cellSelectionInfoCE1***Parameters included in coverage enhancement S criteria for BL UEs and UEs in CE supporting CE Mode B. E-UTRAN includes this IE only in an entry of *InterFreqCarrierFreqList-v1350* or *InterFreqCarrierFreqListExt-v1350* if *cellSelectionInfoCE* is present in the corresponding entry of *InterFreqCarrierFreqList-v1310* or *InterFreqCarrierFreqListExt-v1310* is present. |
| ***freqBandInfo***A list of *additionalPmax* and *additionalSpectrumEmission* values, as defined in TS 36.101 [42], table 6.2.4-1, for UEs neither in CE nor BL UEs, TS 36.101 [42], table 6.2.4E-1, for UEs in CE or BL UEs and TS 36.102 [113], table 6.2A.3-1, for NTN capable UE, for the frequency band represented by *dl-CarrierFreq* for which cell reselection parameters are common. If E-UTRAN includes *freqBandInfo-v10l0* it includes the same number of entries, and listed in the same order, as in *freqBandInfo-r10*. |
| ***hsdn-Indication***Indicates whether there are deployed HSDN cells or not on the the DL carrier frequency indicated by *dl-CarrierFreq-r12*.  |
| ***interFreqCarrierFreqList***List of neighbouring inter-frequencies. E-UTRAN does not configure more than one entry for the same physical frequency regardless of the E-ARFCN used to indicate this. If E-UTRAN includes *interFreqCarrierFreqList-v8h0*, *interFreqCarrierFreqList-v9e0*, *InterFreqCarrierFreqList-v1250, InterFreqCarrierFreqList-v1310, InterFreqCarrierFreqList-v1350,* *InterFreqCarrierFreqList-v13a0*, *InterFreqCarrierFreqList-v1530, InterFreqCarrierFreqList-v1610*, and/or *InterFreqCarrierFreqList-v1800*, it includes the same number of entries, and listed in the same order, as in *interFreqCarrierFreqList* (i.e. without suffix). See Annex D for more descriptions. |
| ***interFreqCarrierFreqListExt***List of additional neighbouring inter-frequencies, i.e. extending the size of the inter-frequency carrier list using the general principles specified in 5.1.2. E-UTRAN does not configure more than one entry for the same physical frequency regardless of the E-ARFCN used to indicate this. EUTRAN may include *interFreqCarrierFreqListExt* even if *interFreqCarrierFreqList* (i.e without suffix) does not include *maxFreq* entries. If E-UTRAN includes *InterFreqCarrierFreqListExt-v1310, InterFreqCarrierFreqListExt-v1350,* *InterFreqCarrierFreqListExt-v1360*, *InterFreqCarrierFreqListExt-v1530, InterFreqCarrierFreqListExt-v1610,* and/or *InterFreqCarrierFreqListExt-v1800*, it includes the same number of entries, and listed in the same order, as in *interFreqCarrierFreqListExt-r12.* |
| ***interFreqExcludedCellList***List of exclude-listed inter-frequency neighbouring cells. |
| ***interFreqNeighCellList***List of inter-frequency neighbouring cells with specific cell re-selection parameters. *interFreqNeighCellList-v1610* indicates list of RSS assistance information which is used for the corresponding *physCellId*. If E-UTRAN includes *interFreqNeighCellList-v1610* in *interFreqCarrierFreqList-v1610 / interFreqCarrierFreqListExt-v1610*, it includes the same number of entries, and listed in the same order, as in *interFreqNeighCellList* (i.e. without suffix) / *interFreqNeighCellList-r12.* If *interFreqNeighCellList-v1610* is absent in *interFreqCarrierFreqList-v1610/ interFreqCarrierFreqListExt-v1610*, measurement based on RSS is not applicable for all the neighbour cells in *interFreqNeighCellList* (i.e. without suffix) / *interFreqNeighCellList-r12*. |
| ***interFreqNeighHSDN-CellList***List of inter-frequency neighbouring HSDN cells as specified in TS 36.304 [4]. |
| ***measIdleConfigSIB***Indicates E-UTRA measurement configuration to be stored and used by the UE while in RRC\_IDLE or RRC\_INACTIVE. |
| ***measIdleConfigSIB-NR***Indicates the NR measurement configuration to be stored and used by the UE while in RRC\_IDLE or RRC\_INACTIVE.  |
| ***multiBandInfoList***Indicates the list of frequency bands in addition to the band represented by dl-CarrierFreq for which cell reselection parameters are common. E-UTRAN indicates at most *maxMultiBands* frequency bands (i.e. the total number of entries across both *multiBandInfoList* and *multiBandInfoList-v9e0* is below this limit). |
| ***multiBandInfoList-v10j0***A list of *additionalPmax* and *additionalSpectrumEmission* values, as defined in TS 36.101 [42], table 6.2.4-1, for UEs neither in CE nor BL UEs, TS 36.101 [42], table 6.2.4E-1, for UEs in CE or BL UEs and TS 36.102 [113], table 6.2A.3-1, for NTN capable UE, for the frequency bands in *multiBandInfoList* (i.e. without suffix) and *multiBandInfoList-v9e0*. If E-UTRAN includes *multiBandInfoList-v10j0*, it includes the same number of entries, and listed in the same order, as in *multiBandInfoList* (i.e. without suffix). If E-UTRAN includes *multiBandInfoList-v10l0* it includes the same number of entries, and listed in the same order, as in *multiBandInfoList-v10j0.* |
| ***p-Max***Value applicable for the neighbouring E-UTRA cells on this carrier frequency. If absent the UE applies the maximum power according to its capability as specified in TS 36.101 [42], clause 6.2.2. This field is ignored by IAB-MT. The IAB-MT applies output power and emissions requirements, as specified in TS 38.174 [107]. |
| ***q-OffsetCell***Parameter "Qoffsets,n" in TS 36.304 [4]. |
| ***q-OffsetFreq***Parameter "Qoffsetfrequency" in TS 36.304 [4]. |
| ***q-QualMin***Parameter "Qqualmin" in TS 36.304 [4]. If the field is not present, the UE applies the (default) value of negative infinity for Qqualmin. NOTE 1. |
| ***q-QualMinRSRQ-OnAllSymbols***If this field is present and supported by the UE, the UE shall, when performing RSRQ measurements, perform RSRQ measurement on all OFDM symbols in accordance with TS 36.214 [48]. NOTE 1. |
| ***q-QualMinWB***If this field is present and supported by the UE, the UE shall, when performing RSRQ measurements, use a wider bandwidth in accordance with TS 36.133 [16]. NOTE 1. |
| ***redistributionFactorFreq***Parameter *redistributionFactorFreq* in TS 36.304 [4]. |
| ***redistributionFactorCell***Parameter *redistributionFactorCell* in TS 36.304 [4]. |
| ***reducedMeasPerformance***Value *TRUE* indicates that the neighbouring inter-frequency is configured for reduced measurement performance, see TS 36.133 [16]. If the field is not included, the neighbouring inter-frequency is configured for normal measurement performance, see TS 36.133 [16].  |
| ***rss-ConfigCarrierInfo***RSS configuration for this carrier frequency. If absent and *rss-MeasConfig* is included in *SIB2*, RSS is collocated (time and frequency domain) in all cells on this carrier. |
| ***satelliteAssistanceInfoList***List of satellite ID(s), used to associate with the satellite assistance information in *SystemInformationBlockType31* and *SystemInformationBlockType33* for neighbour cell measurements on this frequency. Each satellite ID included in this list corresponds to a *satelliteId* configured via *SystemInformationBlockType31* or in *neighSatelliteInfoList* via *SystemInformationBlockType33*. If the field is not present for a frequency and *neighSatelliteInfoList* is broadcast in *SystemInformationBlockType33*, the UE considers the cells on the frequency to be terrestrial cells and UE shall delete any existing value for this field. |
| ***scptm-FreqOffset***Parameter QoffsetSCPTM in TS 36.304 [4]. Actual value QoffsetSCPTM = field value \* 2 [dB]. If the field is not present, the UE uses infinite dBs for the SC-PTM frequency offset with cell ranking as specified in TS 36.304 [4]. |
| ***threshX-High***Parameter "ThreshX, HighP" in TS 36.304 [4]. |
| ***threshX-HighQ***Parameter "ThreshX, HighQ" in TS 36.304 [4]. |
| ***threshX-Low***Parameter "ThreshX, LowP" in TS 36.304 [4]. |
| ***threshX-LowQ***Parameter "ThreshX, LowQ" in TS 36.304 [4]. |
| ***t-ReselectionEUTRA***Parameter "TreselectionEUTRA" in TS 36.304 [4]. |
| ***t-ReselectionEUTRA-SF***Parameter "Speed dependent ScalingFactor for TreselectionEUTRA" in TS 36.304 [4]. If the field is not present, the UE behaviour is specified in TS 36.304 [4]. |

NOTE 1: The value the UE applies for parameter "Qqualmin" in TS 36.304 [4] depends on the *q-QualMin* fields signalled by E-UTRAN and supported by the UE. In case multiple candidate options are available, the UE shall select the highest priority candidate option according to the priority order indicated by the following table (top row is highest priority).

|  |  |  |
| --- | --- | --- |
| q-QualMinRSRQ-OnAllSymbols | q-QualMinWB | Value of parameter "Qqualmin" in TS 36.304 [4] |
| Included | Included | *q-QualMinRSRQ-OnAllSymbols* – (*q-QualMin* – *q-QualMinWB*) |
| Included | Not included | *q-QualMinRSRQ-OnAllSymbols* |
| Not included | Included | *q-QualMinWB* |
| Not included | Not included | *q-QualMin* |

| Conditional presence | Explanation |
| --- | --- |
| *dl-FreqMax* | The field is mandatory present if, for the corresponding entry in *InterFreqCarrierFreqList* (i.e. without suffix), *dl-CarrierFreq* (i.e. without suffix) is set to *maxEARFCN*. Otherwise the field is not present. |
| *QrxlevminCE1* | The field is optionally present, Need OR, if *q-RxLevMinCE1-r13* is set below -140 dBm. Otherwise the field is not present. |
| *RSRQ* | The field is mandatory present if *threshServingLowQ* is present in *systemInformationBlockType3*; otherwise it is not present. |
| *RSRQ2* | The field is mandatory present for all EUTRA carriers listed in SIB5 if *q-QualMinRSRQ-OnAllSymbols* is present in SIB3; otherwise it is not present and the UE shall delete any existing value for this field. |
| *RSS* | This field is optional, need OP, if *rss-MeasConfig* is included in SIB2. Otherwise the field is not present, and the UE shall delete any existing value for this field. |
| *WB-RSRQ* | The field is optionally present, need OP if the measurement bandwidth indicated by *allowedMeasBandwidth* is 50 resource blocks or larger; otherwise it is not present. |

<Irrelevant Texts Omitted>

#### – *SystemInformationBlockType24*

The IE *SystemInformationBlockType24* contains information relevant for inter-RAT cell re-selection (i.e. information about NR frequencies and NR neighbouring cells relevant for cell re-selection), which can also be used for NR idle/inactive measurements. The IE includes cell re-selection parameters common for a frequency.

*SystemInformationBlockType24* information element

-- ASN1START

SystemInformationBlockType24-r15 ::= SEQUENCE {

 carrierFreqListNR-r15 CarrierFreqListNR-r15 OPTIONAL, -- Need OR

 t-ReselectionNR-r15 T-Reselection,

 t-ReselectionNR-SF-r15 SpeedStateScaleFactors OPTIONAL, -- Need OR

 lateNonCriticalExtension OCTET STRING OPTIONAL,

 ...,

 [[ carrierFreqListNR-v1610 CarrierFreqListNR-v1610 OPTIONAL -- Need OR

 ]],

 [[ carrierFreqListNR-v1700 CarrierFreqListNR-v1700 OPTIONAL -- Need OR

 ]],

 [[ carrierFreqListNR-v1720 CarrierFreqListNR-v1720 OPTIONAL -- Need OR

 ]],

 [[ carrierFreqListNR-v1810 CarrierFreqListNR-v1810 OPTIONAL -- Need OR

 ]],

 [[ carrierFreqListNR-v19xy CarrierFreqListNR-v19xy OPTIONAL -- Need OR

 ]]

}

CarrierFreqListNR-r15 ::= SEQUENCE (SIZE (1..maxFreq)) OF CarrierFreqNR-r15

CarrierFreqListNR-v1610 ::= SEQUENCE (SIZE (1..maxFreq)) OF CarrierFreqNR-v1610

CarrierFreqListNR-v1700 ::= SEQUENCE (SIZE (1..maxFreq)) OF CarrierFreqNR-v1700

CarrierFreqListNR-v1720 ::= SEQUENCE (SIZE (1..maxFreq)) OF CarrierFreqNR-v1720

CarrierFreqListNR-v1810 ::= SEQUENCE (SIZE (1..maxFreq)) OF CarrierFreqNR-v1810

CarrierFreqListNR-v19xy ::= SEQUENCE (SIZE (1..maxFreq)) OF CarrierFreqNR-v19xy

CarrierFreqNR-r15 ::= SEQUENCE {

 carrierFreq-r15 ARFCN-ValueNR-r15,

 multiBandInfoList-r15 MultiFrequencyBandListNR-r15 OPTIONAL, -- Need OR

 multiBandInfoListSUL-r15 MultiFrequencyBandListNR-r15 OPTIONAL, -- Need OR

 measTimingConfig-r15 MTC-SSB-NR-r15 OPTIONAL, -- Need OR

 subcarrierSpacingSSB-r15 ENUMERATED {kHz15, kHz30, kHz120, kHz240},

 ss-RSSI-Measurement-r15 SS-RSSI-Measurement-r15 OPTIONAL, -- Cond RSRQ2

 cellReselectionPriority-r15 CellReselectionPriority OPTIONAL, -- Need OP

 cellReselectionSubPriority-r15 CellReselectionSubPriority-r13 OPTIONAL, -- Need OR

 threshX-High-r15 ReselectionThreshold,

 threshX-Low-r15 ReselectionThreshold,

 threshX-Q-r15 SEQUENCE {

 threshX-HighQ-r15 ReselectionThresholdQ-r9,

 threshX-LowQ-r15 ReselectionThresholdQ-r9

 } OPTIONAL, -- Cond RSRQ

 q-RxLevMin-r15 INTEGER (-70..-22),

 q-RxLevMinSUL-r15 INTEGER (-70..-22) OPTIONAL, -- Need OR

 p-MaxNR-r15 P-MaxNR-r15,

 ns-PmaxListNR-r15 NS-PmaxListNR-r15 OPTIONAL, -- Need OR

 q-QualMin-r15 INTEGER (-43..-12) OPTIONAL, -- Need OP

 deriveSSB-IndexFromCell-r15 BOOLEAN,

 maxRS-IndexCellQual-r15 MaxRS-IndexCellQualNR-r15 OPTIONAL, -- Need OR

 threshRS-Index-r15 ThresholdListNR-r15 OPTIONAL, -- Need OR

 ...,

 [[ multiBandNsPmaxListNR-v1550 MultiBandNsPmaxListNR-1-v1550 OPTIONAL, -- Need OR

 multiBandNsPmaxListNR-SUL-v1550 MultiBandNsPmaxListNR-v1550 OPTIONAL, -- Need OR

 ssb-ToMeasure-r15 SSB-ToMeasure-r15 OPTIONAL -- Need OR

 ]],

 [[ ns-PmaxListNR-v1760 NS-PmaxListNR-v1760 OPTIONAL, -- Need OR

 multiBandNsPmaxListNR-v1760 MultiBandNsPmaxListNR-1-v1760 OPTIONAL, -- Need OR

 multiBandNsPmaxListNR-SUL-v1760 MultiBandNsPmaxListNR-v1760 OPTIONAL -- Need OR

 ]]

}

CarrierFreqNR-v1610 ::= SEQUENCE {

 smtc2-LP-r16 MTC-SSB2-LP-NR-r16 OPTIONAL, -- Need OR

 ssb-PositionQCL-CommonNR-r16 SSB-PositionQCL-RelationNR-r16 OPTIONAL, -- Cond SharedSpectrum2

 allowedCellListNR-r16 AllowedCellListNR-r16 OPTIONAL, -- Cond SharedSpectrum

 highSpeedCarrierNR-r16 ENUMERATED {true} OPTIONAL -- Need OR

}

CarrierFreqNR-v1700 ::= SEQUENCE {

 nr-FreqNeighHSDN-CellList-r17 NR-FreqNeighHSDN-CellList-r17 OPTIONAL -- Need OR

}

CarrierFreqNR-v1720 ::= SEQUENCE {

 subcarrierSpacingSSB-r17 ENUMERATED {kHz480, spare1} OPTIONAL, -- Need OR

 ssb-PositionQCL-CommonNR-r17 SSB-PositionQCL-RelationNR-r17 OPTIONAL -- Cond SharedSpectrum2

}

CarrierFreqNR-v1810 ::= SEQUENCE {

 carrierFreq-r18 ARFCN-ValueNR-r15 OPTIONAL, -- Cond LessThan5MHz

 multiBandInfoList-r18 MultiFrequencyBandListNR-r15 OPTIONAL, -- Cond LessThan5MHz

 multiBandInfoListAerial-r18 MultiFrequencyBandListNR-r15 OPTIONAL, -- Need OR

 ns-PmaxListNR-Aerial-r18 NS-PmaxListNR-Aerial-r18 OPTIONAL, -- Need OR

 multiBandNsPmaxListNR-Aerial-r18 MultiBandNsPmaxListNR-Aerial-1-r18 OPTIONAL, -- Need OR

 mobileIAB-CellList-r18 PhysCellIdRangeNR-r16 OPTIONAL, -- Need OR

 mobileIAB-Freq-r18 ENUMERATED {true} OPTIONAL -- Need OR

}

CarrierFreqNR-v19xy ::= SEQUENCE {

 satAssistanceInfoList-r19 SEQUENCE (SIZE(1..maxSat-r17)) OF SatelliteId-r18 OPTIONAL -- Need OR

}

MultiBandNsPmaxListNR-1-v1550 ::= SEQUENCE (SIZE (1.. maxMultiBandsNR-1-r15)) OF NS-PmaxListNR-r15

MultiBandNsPmaxListNR-v1550 ::= SEQUENCE (SIZE (1.. maxMultiBandsNR-r15)) OF NS-PmaxListNR-r15

MultiBandNsPmaxListNR-1-v1760 ::= SEQUENCE (SIZE (1.. maxMultiBandsNR-1-r15)) OF NS-PmaxListNR-v1760

MultiBandNsPmaxListNR-v1760 ::= SEQUENCE (SIZE (1.. maxMultiBandsNR-r15)) OF NS-PmaxListNR-v1760

MultiBandNsPmaxListNR-Aerial-1-r18 ::= SEQUENCE (SIZE (1.. maxMultiBandsNR-1-r15)) OF NS-PmaxListNR-Aerial-r18

AllowedCellListNR-r16 ::= SEQUENCE (SIZE (1..maxCellAllowedNR-r16)) OF PhysCellIdNR-r15

NR-FreqNeighHSDN-CellList-r17 ::= SEQUENCE (SIZE (1..maxCellNR-r17)) OF PhysCellIdRangeNR-r16

-- ASN1STOP

|  |
| --- |
| *SystemInformationBlockType24* field descriptions |
| ***allowedCellListNR***List of allow-listed neighbouring NR cells. |
| ***carrierFreqListNR***List of carrier frequencies of NR carriers. These frequencies correspond to GSCN values as specified in TS 38.101 [85]. If the *carrierFreqListNR-v1610, carrierFreqListNR-v1700*, *carrierFreqListNR-v1720*, *carrierFreqListNR-v1810* or *carrierFreqListNR-v19xy* is present, it contains the same number of entries, listed in the same order as in the *carrierFreqListNR* (without suffix).For a neighbouring carrier frequency when *carrierFreq-r18* is included, the network sets the corresponding value of *carrierFreq-r15* to 250, and the UE applies *carrierFreq-r18* instead of *carrierFreq-r15*. In such case, if the UE does not support the GSCN value corresponding to the *carrierFreq-r18*, it ignores the corresponding neighbour cell. |
| ***cellReselectionPriority***The field concerns the absolute priority of the concerned carrier frequency as used by the cell reselection procedure. Corresponds with parameter "priority" in TS 36.304 [4]. |
| ***deriveSSB-IndexFromCell***The field indicates whether the UE may use, to derive the SSB index of a cell on the indicated SSB frequency and subcarrier spacing, the timing of any detected cell with the same SSB frequency and subcarrier spacing. If this field is set to TRUE, the UE assumes SFN and frame boundary alignment across cells on the same NR carrier frequency as specified in TS 36.133 [16]. |
| ***highSpeedCarrierNR***If the field is present, the UE shall apply the enhanced inter-RAT NR measurement requirements to support high speed up to 500 km/h as specified in TS 36.133 [16] to the NR carrier. |
| ***maxRS-IndexCellQual***Number of SS blocks to average for cell measurement derivation. Corresponds to the parameter *nrofSS-BlocksToAverage* in TS 38.304 [92]. |
| ***measTimingConfig***Used to configure measurement timing configurations, i.e., timing occasions at which the UE measures SSBs. If the field is absent, the UE assumes that SSB periodicity is 5ms in this frequency. If field *satAssistanceInfoList* is configured for the corresponding entry, the *offset* (derived from parameter *periodicityAndOffset*) is based on the assumption that the UE's propagation delay difference between serving cell and neighbour cells equals to 0 ms, and UE can adjust the offset based on the actual propagation delay. |
| ***mobileIAB-CellList***List of neighbouring mobile IAB cells as specified in TS 36.304 [4]. |
| ***mobileIAB-Freq***If present, it indicates that a mobile IAB node may be deployed on the NR frequency.  |
| ***multiBandInfoList***Indicates the list of frequency bands for which the NR cell reselection parameters apply. The UE shall select the first listed band which it supports in the *multiBandInfoList* field to represent the NR neighbour carrier frequency. The network always includes *multiBandInfoList-r15*.For a neighbouring carrier frequency when *multiBandInfoList-r18* is included, the network sets the corresponding value of *FreqBandIndicatorNR-r15* in *multiBandInfoList-r15* to 200, and the UE applies *multBandInfoList-r18* instead of *multiBandInfoList-r15*. |
| ***multiBandInfoListAerial***Indicates the list of frequency bands for which the NR cell reselection parameters apply. The aerial UE shall select the first listed band which it supports in the *multiBandInfoListAerial* field to represent the NR neighbour carrier frequency. |
| ***multiBandInfoListSUL***Indicates the list of frequency bands for which the NR cell reselection parameters apply. The UE shall select the first listed band which it supports in the *multiBandInfoListSUL* field to represent the NR neighbour carrier frequency. |
| ***multiBandNsPmaxListNR***Indicates the *NS-PmaxListNR* configuration for the NR frequency band(s) listed in *multiBandInfoList*. The first entry corresponds to the second listed band in *multiBandInfoList*, and second entry corresponds to the third listed band in *multiBandInfoList*, and so on.  |
| ***multiBandNsPmaxListNR-Aerial***Indicates the *NS-PmaxListNR-Aerial* configuration for the NR frequency band(s) listed in *multiBandInfoListAerial*. The first entry corresponds to the second listed band in *multiBandInfoListAerial*, and second entry corresponds to the third listed band in *multiBandInfoListAerial*, and so on. |
| ***multiBandNsPmaxListNR-SUL***Indicates the *NS-PmaxListNR* configuration for the NR SUL frequency band(s) listed in *multiBandInfoListSUL*. The first entry corresponds to the first listed band in *multiBandInfoListSUL*, and second entry corresponds to the second listed band in *multiBandInfoListSUL*, and so on. |
| ***nr-FreqNeighHSDN-CellList***List of neighbouring NR HSDN cells as specified in TS 38.304 [92]. |
| ***ns-PmaxListNR***Indicates a list of *additionalPmax* and *additionalSpectrumEmission*, corresponds to the first listed band in the *multiBandInfoList*. |
| ***ns-PmaxListNR-Aerial***Indicates a list of *additionalPmax* and *additionalSpectrumEmission* for aerial UE, corresponds to the first listed band in the *multiBandInfoListAerial*. |
| ***p-MaxNR***Indicates the maximum power for NR (see TS 38.104 [91]). |
| ***q-QualMin***Parameter "Qqualmin" in TS 36.304 [4], applicable for NR neighbour cells. If the field is not present, the UE applies the (default) value of negative infinity for Qqualmin. The actual value Qqualmin = field value [dB]. |
| ***q-RxLevMin***Parameter "Qrxlevmin" in TS 38.304 [92], applicable for NR neighbour cells. The actual value Qrxlevmin = field value \* 2 [dBm]. |
| ***q-RxLevMinSUL***Parameter "Qrxlevmin" in TS 38.304 [92], applicable for NR neighbouring cells. The actual value Qrxlevmin = field value \* 2 [dBm]. |
| ***satAssistanceInfoList***List of satellite ID(s), used to associate with the satellite assistance information for neighbour cell measurements on this frequency. Each satellite ID included in this list corresponds to a *satelliteId* configured in *neighSatelliteInfoListNR* via *SystemInformationBlockType33*. If the field is not present for a frequency and *neighSatelliteInfoListNR* is broadcast in *SystemInformationBlockType33*, the UE considers the cells on the frequency to be terrestrial cells. |
| ***smtc2-LP***Measurement timing configuration for inter-RAT neighbour cells in NR with a Long Periodicity (LP) indicated by periodicity in *smtc2-LP*. The timing offset and duration are equal to the offset and duration indicated in *measTimingConfig* in *CarrierFreqNR*. The periodicity in *smtc2-LP* can only be set to a value strictly larger than the periodicity in *measTimingConfig* in *CarrierFreqNR* (e.g. if *measTimingConfig* indicates sf20 the Long Periodicity can only be set to sf40, sf80 or sf160, if *measTimingConfig* indicates sf160, *smtc2-LP* cannot be configured). The *pci-List*, if present, includes the physical cell identities of the inter-RAT neighbour cells with Long Periodicity. If *smtc2-LP* is absent, the UE assumes that there are no inter-RAT neighbour cells with a Long Periodicity. |
| ***ssb-PositionQCL-CommonNR***Indicates the QCL relationship between SS/PBCH blocks for NR neighbor cells on the indicated frequency as specified in TS 38.213 [88], clause 4.1. If *ssb-PositionQCL-CommonNR-r17* is present, the UE ignores *ssb-PositionQCL-CommonNR-r16*. |
| ***ssb-ToMeasure***The set of SS blocks to be measured within the SMTC measurement duration (see TS 38.215 [89]). When the field is absent the UE measures on all SS-blocks. |
| ***ss-RSSI-Measurements***Indicates the SSB-based RSSI measurement configuration. If the field is absent, the UE behaviour is defined in TS 38.215 [89], clause 5.1.3. |
| ***subcarrierSpacingSSB***Indicates the subcarrier spacing of SSB of NR frequency. Only the values 15 kHz or 30 kHz (FR1), 120 kHz or 240 kHz (FR2-1), 120 kHz or 480 kHz (FR2-2) are applicable. If *subcarrierSpacingSSB-r17* is present, the UE ignores *subcarrierSpacingSSB-r15*. |
| ***threshRS-Index***List of thresholds for consolidation of L1 measurements per RS index. Corresponds to the parameter *absThreshSS-BlocksConsolidation* in TS 38.304 [92]. |
| ***threshX-High***Parameter "ThreshX, HighP" in TS 36.304 [4]. |
| ***threshX-HighQ***Parameter "ThreshX, HighQ" in TS 36.304 [4]. |
| ***threshX-Low***Parameter "ThreshX, LowP" in TS 36.304 [4]. |
| ***threshX-LowQ***Parameter "ThreshX, LowQ" in TS 36.304 [4]. |
| ***t-ReselectionNR***Parameter "TreselectionNR" in TS 36.304 [4]. |
| ***t-ReselectionNR-SF***Parameter "Speed dependent ScalingFactor for TreselectionNR" in TS 36.304 [4]. If the field is not present, the UE behaviour is specified in TS 36.304 [4]. |

| Conditional presence | Explanation |
| --- | --- |
| *LessThan5MHz* | The field is mandatory present if the NR neighbor cell supports 12 PRB, 15 PRB or 20 PRB transmission bandwidth configuration as defined in TS 38.101-1 [85], TS 38.211 [117] and TS 38.213 [88]. Otherwise, the field is not present and the corresponding Rel-15 field applies. |
| *RSRQ* | The field is mandatory present if the *threshServingLowQ* is present in *systemInformationBlockType3*; otherwise it is not present. |
| *RSRQ2* | The field is optional Need OP if the *threshServingLowQ* is present in *systemInformationBlockType3*; otherwise it is not present. |
| *SharedSpectrum* | The field is optional Need OP if NR operates with shared spectrum channel access; otherwise, it is not present. |
| *SharedSpectrum2* | The field is mandatory present if NR operates with shared spectrum channel access; otherwise, it is not present. |

<Irrelevant Texts Omitted>

#### – *SystemInformationBlockType33*

The IE *SystemInformationBlockType33* contains satellite assistance information for neighbour cells.

*SystemInformationBlockType33* information element

-- ASN1START

SystemInformationBlockType33-r18 ::= SEQUENCE {

 neighSatelliteInfoList-r18 NeighSatelliteInfoList-r18 OPTIONAL, -- Need OR

 neighValidityDuration-r18 ENUMERATED {s5, s10, s15, s20, s25, s30, s35, s40,

 s45, s50, s55, s60, s120, s180, s240, s900}

 OPTIONAL, -- Need OP

 lateNonCriticalExtension OCTET STRING OPTIONAL,

 ...,

 [[

 neighSatelliteInfoListNR-r19 NeighSatelliteInfoListNR-r19 OPTIONAL -- Need OR

 ]]

}

NeighSatelliteInfoListNR-r19 ::= SEQUENCE (SIZE(1..maxSat-r17)) OF NeighSatelliteInfoNR-r19

NeighSatelliteInfoList-r18 ::= SEQUENCE (SIZE(1..maxSat-r17)) OF NeighSatelliteInfo-r18

NeighSatelliteInfo-r18 ::= SEQUENCE {

 satelliteId-r18 SatelliteId-r18,

 ephemerisInfo-r18 CHOICE {

 stateVectors-r18 EphemerisStateVectors-r17,

 orbitalParameters-r18 EphemerisOrbitalParameters-r17

 },

 nta-CommonParameters-r18 SEQUENCE {

 nta-Common-r18 INTEGER (0..8316827) OPTIONAL, -- Need OP

 nta-CommonDrift-r18 INTEGER (-261935..261935) OPTIONAL, -- Need OP

 nta-CommonDriftVariation-r18 INTEGER (0..29479) OPTIONAL -- Need OP

 },

 epochTime-r18 SEQUENCE {

 startSFN-r18 INTEGER (0..1023),

 startSubFrame-r18 INTEGER (0..9)

 } OPTIONAL, -- Need OP

 k-Mac-r18 INTEGER (1..512) OPTIONAL, -- Need OP

 t-ServiceStartNeigh-r18 TimeOffsetUTC-r17 OPTIONAL -- Need OR

}

NeighSatelliteInfoNR-r19::= SEQUENCE {

 satelliteId-r19 SatelliteId-r18,

 ephemerisInfo-r19 CHOICE {

 stateVectors-r19 EphemerisStateVectors-r17,

 orbitalParameters-r19 EphemerisOrbitalParameters-r17

 } OPTIONAL, -- Need OP

 nta-CommonParametersNR-r19 SEQUENCE {

 nta-CommonNR-r19 INTEGER (0.. 66485757) OPTIONAL, -- Need OP

 nta-CommonDriftNR-r19 INTEGER (-257303..257303) OPTIONAL, -- Need OP

 nta-CommonDriftVariationNR-r19 INTEGER (0..28949) OPTIONAL -- Need OP

 },

 epochTime-r19 SEQUENCE {

 startSFN-r19 INTEGER (0..1023),

 startSubFrame-r19 INTEGER (0..9)

 } OPTIONAL, -- Need OP

 k-Mac-r19 INTEGER (1..512) OPTIONAL, -- Need OP

 ntn-PolarizationDL-r19 ENUMERATED {rhcp,lhcp,linear} OPTIONAL -- Need OR

}

-- ASN1STOP

|  |
| --- |
| *SystemInformationBlockType33* field descriptions |
| ***ephemerisInfo***Ephemeris data for a neighbour NR NTN satellite (if included in *NeighSatelliteInfoNR*). This field is mandatory present in *NeighSatelliteInfoNR*, if the *satelliteId* in the same entry of *neighSatelliteInfoListNR* does not match any *satelliteId* values included in *neighSatelliteInfoList*. If this field is absent in *NeighSatelliteInfoNR* and the *satelliteId* in the same entry of *neighSatelliteInfoListNR* equals a *satelliteId* value included in *neighSatelliteInfoList*, UE uses the *ephemerisInfo* identified by that *satelliteId* in the *neighSatelliteInfoList.* |
| ***epochTime***Epoch time of the neighbour satellite ephemeris data and common TA parameters, see TS 36.213 [23]. The reference point for epoch time of the neighbour satellite ephemeris and Common TA parameters is the uplink time synchronization reference point of the serving cell when this field is provided in an NTN cell and the eNB when this field is provided in a TN cell.*epochTime* is the starting time of a DL subframe indicated by *startSFN* and *startSubframe*. If this field is absent in an NTN cell, the UE uses epoch time of the serving cell, otherwise the field is based on the timing of the serving cell, i.e. the SFN and sub-frame number indicated in this field refers to the SFN and sub-frame of the serving cell. *The startSFN* indicates the SFN nearest to the frame where the message indicating the *epochTime* is received. If this field is absent in a TN cell, the epoch time is the starting time of the DL subframe corresponding to the end of the SI window during which the SI message carrying SIB33(-NB) is transmitted. |
| ***k-Mac***Scheduling offset used when downlink and uplink frame timing are not aligned at the eNB, see TS 36.213 [23]. Unit in ms.If the field if absent, the UE uses the (default) value of 0. |
| ***neighSatelliteInfoListNR***Indicates a list of satellites providing NR NTN neighbor cells. This field is only included in a TN cell. |
| ***neighValidityDuration***Validity duration of the neighbour satellite ephemeris data and common TA parameters, i.e. maximum time duration (from *epochTime*) during which the UE can apply the satellite ephemeris without acquiring new satellite ephemeris, see TS 36.213 [23]. Unit in second.Value *s5* corresponds to 5 seconds, value *s10* corresponds to 10 seconds and so on.If this field is absent in an NTN cell, the UE uses validity duration from the serving cell assistance information. If this field is absent in a TN cell, how the UE sets validity duration is left to UE implementation. |
| ***nta-Common, nta-CommonNR***Network-controlled common TA, see TS 36.213 [23]. Unit of μs.For *nta-Common*, step of 32.55208 ×10-3 μs. For *nta-CommonNR*, step of 4.072 × 10-3μs. Actual value = field value \* step.If the field is absent, the UE uses the (default) value of 0. |
| ***nta-CommonDrift, nta-CommonDriftNR***Drift rate of the common TA, see TS 36.213 [23]. Unit of μs/s.Step of 0.2 ×10-3 μs/s. Actual value = field value \* 0.2 ×10-3.If the field is absent, the UE uses the (default) value of 0. |
| ***nta-CommonDriftVariation, nta-CommonDriftVariationNR***Drift rate variation of the common TA, see TS 36.213 [23]. Unit of μs/s2.Step of 0.2 ×10-4 μs/s2. Actual value = field value \* 0.2 ×10-4.If the field is absent, the UE uses the (default) value of 0. |
| ***ntn-PolarizationDL***If present, this parameter indicates polarization information for downlink transmission on service link of a satellite for NR NTN: including Right hand, Left hand circular polarizations (RHCP, LHCP) and Linear polarization. |
| ***t-ServiceStartNeigh***Indicates the earliest time when the area covered by the current serving cell is going to be covered by the neighbour cell(s) served by the satellite indicated by *satelliteId*, see 5.5.3.1, 5.5.8 and 36.304 [4]. This field is only present for the NTN quasi-Earth fixed neighbour cell(s). |

|  |
| --- |
| Next change |

### 6.3.4 Mobility control information elements

<Irrelevant Texts Omitted>

#### – *FreqBandIndicatorNR*

The IE *FreqBandIndicatorNR* indicates the NR operating band as defined in TS 38.101-1 [85] and TS 38.101-5 [116].

*FreqBandIndicatorNR* information element

-- ASN1START

FreqBandIndicatorNR-r15 ::= INTEGER (1.. maxFBI-NR-r15)

-- ASN1STOP

<Irrelevant Texts Omitted>

|  |
| --- |
| Next change |

### 6.3.6 Other information elements

<Irrelevant Texts Omitted>

#### – *SatelliteId*

The IE *SatelliteId* is used to identify the satellite assistance information of the serving satellite, or neighbour satellites for E-UTRA and/or NR.

*SatelliteId* information element

-- ASN1START

SatelliteId-r18 ::= INTEGER (0..255)

-- ASN1STOP

<Irrelevant Texts Omitted>

#### – *UE-EUTRA-Capability*

The IE *UE-EUTRA-Capability* is used to convey the E-UTRA UE Radio Access Capability Parameters, see TS 36.306 [5], and the Feature Group Indicators for mandatory features (defined in Annexes B.1 and C.1) to the network. The IE *UE-EUTRA-Capability* is transferred in E-UTRA or in another RAT.

NOTE 0: For (UE capability specific) guidelines on the use of keyword OPTIONAL, see Annex A.3.5.

*UE-EUTRA-Capability* information element

-- ASN1START

UE-EUTRA-Capability ::= SEQUENCE {

 accessStratumRelease AccessStratumRelease,

 ue-Category INTEGER (1..5),

 pdcp-Parameters PDCP-Parameters,

 phyLayerParameters PhyLayerParameters,

 rf-Parameters RF-Parameters,

 measParameters MeasParameters,

 featureGroupIndicators BIT STRING (SIZE (32)) OPTIONAL,

 interRAT-Parameters SEQUENCE {

 utraFDD IRAT-ParametersUTRA-FDD OPTIONAL,

 utraTDD128 IRAT-ParametersUTRA-TDD128 OPTIONAL,

 utraTDD384 IRAT-ParametersUTRA-TDD384 OPTIONAL,

 utraTDD768 IRAT-ParametersUTRA-TDD768 OPTIONAL,

 geran IRAT-ParametersGERAN OPTIONAL,

 cdma2000-HRPD IRAT-ParametersCDMA2000-HRPD OPTIONAL,

 cdma2000-1xRTT IRAT-ParametersCDMA2000-1XRTT OPTIONAL

 },

 nonCriticalExtension UE-EUTRA-Capability-v920-IEs OPTIONAL

}

-- Late non critical extensions

UE-EUTRA-Capability-v9a0-IEs ::= SEQUENCE {

 featureGroupIndRel9Add-r9 BIT STRING (SIZE (32)) OPTIONAL,

 fdd-Add-UE-EUTRA-Capabilities-r9 UE-EUTRA-CapabilityAddXDD-Mode-r9 OPTIONAL,

 tdd-Add-UE-EUTRA-Capabilities-r9 UE-EUTRA-CapabilityAddXDD-Mode-r9 OPTIONAL,

 nonCriticalExtension UE-EUTRA-Capability-v9c0-IEs OPTIONAL

}

UE-EUTRA-Capability-v9c0-IEs ::= SEQUENCE {

 interRAT-ParametersUTRA-v9c0 IRAT-ParametersUTRA-v9c0 OPTIONAL,

 nonCriticalExtension UE-EUTRA-Capability-v9d0-IEs OPTIONAL

}

UE-EUTRA-Capability-v9d0-IEs ::= SEQUENCE {

 phyLayerParameters-v9d0 PhyLayerParameters-v9d0 OPTIONAL,

 nonCriticalExtension UE-EUTRA-Capability-v9e0-IEs OPTIONAL

}

UE-EUTRA-Capability-v9e0-IEs ::= SEQUENCE {

 rf-Parameters-v9e0 RF-Parameters-v9e0 OPTIONAL,

 nonCriticalExtension UE-EUTRA-Capability-v9h0-IEs OPTIONAL

}

UE-EUTRA-Capability-v9h0-IEs ::= SEQUENCE {

 interRAT-ParametersUTRA-v9h0 IRAT-ParametersUTRA-v9h0 OPTIONAL,

 -- Following field is only to be used for late REL-9 extensions

 lateNonCriticalExtension OCTET STRING OPTIONAL,

 nonCriticalExtension UE-EUTRA-Capability-v10c0-IEs OPTIONAL

}

UE-EUTRA-Capability-v10c0-IEs ::= SEQUENCE {

 otdoa-PositioningCapabilities-r10 OTDOA-PositioningCapabilities-r10 OPTIONAL,

 nonCriticalExtension UE-EUTRA-Capability-v10f0-IEs OPTIONAL

}

UE-EUTRA-Capability-v10f0-IEs ::= SEQUENCE {

 rf-Parameters-v10f0 RF-Parameters-v10f0 OPTIONAL,

 nonCriticalExtension UE-EUTRA-Capability-v10i0-IEs OPTIONAL

}

UE-EUTRA-Capability-v10i0-IEs ::= SEQUENCE {

 rf-Parameters-v10i0 RF-Parameters-v10i0 OPTIONAL,

 -- Following field is only to be used for late REL-10 extensions

 lateNonCriticalExtension OCTET STRING (CONTAINING UE-EUTRA-Capability-v10j0-IEs) OPTIONAL,

 nonCriticalExtension UE-EUTRA-Capability-v11d0-IEs OPTIONAL

}

UE-EUTRA-Capability-v10j0-IEs ::= SEQUENCE {

 rf-Parameters-v10j0 RF-Parameters-v10j0 OPTIONAL,

 nonCriticalExtension SEQUENCE {} OPTIONAL

}

UE-EUTRA-Capability-v11d0-IEs ::= SEQUENCE {

 rf-Parameters-v11d0 RF-Parameters-v11d0 OPTIONAL,

 otherParameters-v11d0 Other-Parameters-v11d0 OPTIONAL,

 nonCriticalExtension UE-EUTRA-Capability-v11x0-IEs OPTIONAL

}

UE-EUTRA-Capability-v11x0-IEs ::= SEQUENCE {

 -- Following field is only to be used for late REL-11 extensions

 lateNonCriticalExtension OCTET STRING OPTIONAL,

 nonCriticalExtension UE-EUTRA-Capability-v12b0-IEs OPTIONAL

}

UE-EUTRA-Capability-v12b0-IEs ::= SEQUENCE {

 rf-Parameters-v12b0 RF-Parameters-v12b0 OPTIONAL,

 nonCriticalExtension UE-EUTRA-Capability-v12x0-IEs OPTIONAL

}

UE-EUTRA-Capability-v12x0-IEs ::= SEQUENCE {

 -- Following field is only to be used for late REL-12 extensions

 lateNonCriticalExtension OCTET STRING OPTIONAL,

 nonCriticalExtension UE-EUTRA-Capability-v1370-IEs OPTIONAL

}

UE-EUTRA-Capability-v1370-IEs ::= SEQUENCE {

 ce-Parameters-v1370 CE-Parameters-v1370 OPTIONAL,

 fdd-Add-UE-EUTRA-Capabilities-v1370 UE-EUTRA-CapabilityAddXDD-Mode-v1370 OPTIONAL,

 tdd-Add-UE-EUTRA-Capabilities-v1370 UE-EUTRA-CapabilityAddXDD-Mode-v1370 OPTIONAL,

 nonCriticalExtension UE-EUTRA-Capability-v1380-IEs OPTIONAL

}

UE-EUTRA-Capability-v1380-IEs ::= SEQUENCE {

 rf-Parameters-v1380 RF-Parameters-v1380 OPTIONAL,

 ce-Parameters-v1380 CE-Parameters-v1380,

 fdd-Add-UE-EUTRA-Capabilities-v1380 UE-EUTRA-CapabilityAddXDD-Mode-v1380,

 tdd-Add-UE-EUTRA-Capabilities-v1380 UE-EUTRA-CapabilityAddXDD-Mode-v1380,

 nonCriticalExtension UE-EUTRA-Capability-v1390-IEs OPTIONAL

}

UE-EUTRA-Capability-v1390-IEs ::= SEQUENCE {

 rf-Parameters-v1390 RF-Parameters-v1390 OPTIONAL,

 nonCriticalExtension UE-EUTRA-Capability-v13e0a-IEs OPTIONAL

}

UE-EUTRA-Capability-v13e0a-IEs ::= SEQUENCE {

 lateNonCriticalExtension OCTET STRING (CONTAINING UE-EUTRA-Capability-v13e0b-IEs) OPTIONAL,

 nonCriticalExtension UE-EUTRA-Capability-v1470-IEs OPTIONAL

}

UE-EUTRA-Capability-v13e0b-IEs ::= SEQUENCE {

 phyLayerParameters-v13e0 PhyLayerParameters-v13e0,

 -- Following field is only to be used for late REL-13 extensions

 nonCriticalExtension SEQUENCE {} OPTIONAL

}

UE-EUTRA-Capability-v1470-IEs ::= SEQUENCE {

 mbms-Parameters-v1470 MBMS-Parameters-v1470 OPTIONAL,

 phyLayerParameters-v1470 PhyLayerParameters-v1470 OPTIONAL,

 rf-Parameters-v1470 RF-Parameters-v1470 OPTIONAL,

 nonCriticalExtension UE-EUTRA-Capability-v14a0-IEs OPTIONAL

}

UE-EUTRA-Capability-v14a0-IEs ::= SEQUENCE {

 phyLayerParameters-v14a0 PhyLayerParameters-v14a0,

 nonCriticalExtension UE-EUTRA-Capability-v14b0-IEs OPTIONAL

}

UE-EUTRA-Capability-v14b0-IEs ::= SEQUENCE {

 rf-Parameters-v14b0 RF-Parameters-v14b0 OPTIONAL,

 nonCriticalExtension UE-EUTRA-Capability-v14x0-IEs OPTIONAL

}

UE-EUTRA-Capability-v14x0-IEs ::= SEQUENCE {

 -- Following field is only to be used for late REL-14 extensions

 lateNonCriticalExtension OCTET STRING OPTIONAL,

 nonCriticalExtension UE-EUTRA-Capability-v15x0-IEs OPTIONAL

}

UE-EUTRA-Capability-v15x0-IEs ::= SEQUENCE {

 -- Following field is only to be used for late REL-15 extensions

 lateNonCriticalExtension OCTET STRING OPTIONAL,

 nonCriticalExtension UE-EUTRA-Capability-v16c0-IEs OPTIONAL

}

UE-EUTRA-Capability-v16c0-IEs ::= SEQUENCE {

 measParameters-v16c0 MeasParameters-v16c0,

 -- Following field is only to be used for late REL-16 extensions

 lateNonCriticalExtension OCTET STRING OPTIONAL,

 nonCriticalExtension UE-EUTRA-Capability-v17b0-IEs OPTIONAL

}

UE-EUTRA-Capability-v17b0-IEs ::= SEQUENCE {

 ul-RRC-MaxCapaSegments-r17 ENUMERATED {supported} OPTIONAL,

 nonCriticalExtension SEQUENCE {} OPTIONAL

}

-- Regular non critical extensions

UE-EUTRA-Capability-v920-IEs ::= SEQUENCE {

 phyLayerParameters-v920 PhyLayerParameters-v920,

 interRAT-ParametersGERAN-v920 IRAT-ParametersGERAN-v920,

 interRAT-ParametersUTRA-v920 IRAT-ParametersUTRA-v920 OPTIONAL,

 interRAT-ParametersCDMA2000-v920 IRAT-ParametersCDMA2000-1XRTT-v920 OPTIONAL,

 deviceType-r9 ENUMERATED {noBenFromBatConsumpOpt} OPTIONAL,

 csg-ProximityIndicationParameters-r9 CSG-ProximityIndicationParameters-r9,

 neighCellSI-AcquisitionParameters-r9 NeighCellSI-AcquisitionParameters-r9,

 son-Parameters-r9 SON-Parameters-r9,

 nonCriticalExtension UE-EUTRA-Capability-v940-IEs OPTIONAL

}

UE-EUTRA-Capability-v940-IEs ::= SEQUENCE {

 lateNonCriticalExtension OCTET STRING (CONTAINING UE-EUTRA-Capability-v9a0-IEs) OPTIONAL,

 nonCriticalExtension UE-EUTRA-Capability-v1020-IEs OPTIONAL

}

UE-EUTRA-Capability-v1020-IEs ::= SEQUENCE {

 ue-Category-v1020 INTEGER (6..8) OPTIONAL,

 phyLayerParameters-v1020 PhyLayerParameters-v1020 OPTIONAL,

 rf-Parameters-v1020 RF-Parameters-v1020 OPTIONAL,

 measParameters-v1020 MeasParameters-v1020 OPTIONAL,

 featureGroupIndRel10-r10 BIT STRING (SIZE (32)) OPTIONAL,

 interRAT-ParametersCDMA2000-v1020 IRAT-ParametersCDMA2000-1XRTT-v1020 OPTIONAL,

 ue-BasedNetwPerfMeasParameters-r10 UE-BasedNetwPerfMeasParameters-r10 OPTIONAL,

 interRAT-ParametersUTRA-TDD-v1020 IRAT-ParametersUTRA-TDD-v1020 OPTIONAL,

 nonCriticalExtension UE-EUTRA-Capability-v1060-IEs OPTIONAL

}

UE-EUTRA-Capability-v1060-IEs ::= SEQUENCE {

 fdd-Add-UE-EUTRA-Capabilities-v1060 UE-EUTRA-CapabilityAddXDD-Mode-v1060 OPTIONAL,

 tdd-Add-UE-EUTRA-Capabilities-v1060 UE-EUTRA-CapabilityAddXDD-Mode-v1060 OPTIONAL,

 rf-Parameters-v1060 RF-Parameters-v1060 OPTIONAL,

 nonCriticalExtension UE-EUTRA-Capability-v1090-IEs OPTIONAL

}

UE-EUTRA-Capability-v1090-IEs ::= SEQUENCE {

 rf-Parameters-v1090 RF-Parameters-v1090 OPTIONAL,

 nonCriticalExtension UE-EUTRA-Capability-v1130-IEs OPTIONAL

}

UE-EUTRA-Capability-v1130-IEs ::= SEQUENCE {

 pdcp-Parameters-v1130 PDCP-Parameters-v1130,

 phyLayerParameters-v1130 PhyLayerParameters-v1130 OPTIONAL,

 rf-Parameters-v1130 RF-Parameters-v1130,

 measParameters-v1130 MeasParameters-v1130,

 interRAT-ParametersCDMA2000-v1130 IRAT-ParametersCDMA2000-v1130,

 otherParameters-r11 Other-Parameters-r11,

 fdd-Add-UE-EUTRA-Capabilities-v1130 UE-EUTRA-CapabilityAddXDD-Mode-v1130 OPTIONAL,

 tdd-Add-UE-EUTRA-Capabilities-v1130 UE-EUTRA-CapabilityAddXDD-Mode-v1130 OPTIONAL,

 nonCriticalExtension UE-EUTRA-Capability-v1170-IEs OPTIONAL

}

UE-EUTRA-Capability-v1170-IEs ::= SEQUENCE {

 phyLayerParameters-v1170 PhyLayerParameters-v1170 OPTIONAL,

 ue-Category-v1170 INTEGER (9..10) OPTIONAL,

 nonCriticalExtension UE-EUTRA-Capability-v1180-IEs OPTIONAL

}

UE-EUTRA-Capability-v1180-IEs ::= SEQUENCE {

 rf-Parameters-v1180 RF-Parameters-v1180 OPTIONAL,

 mbms-Parameters-r11 MBMS-Parameters-r11 OPTIONAL,

 fdd-Add-UE-EUTRA-Capabilities-v1180 UE-EUTRA-CapabilityAddXDD-Mode-v1180 OPTIONAL,

 tdd-Add-UE-EUTRA-Capabilities-v1180 UE-EUTRA-CapabilityAddXDD-Mode-v1180 OPTIONAL,

 nonCriticalExtension UE-EUTRA-Capability-v11a0-IEs OPTIONAL

}

UE-EUTRA-Capability-v11a0-IEs ::= SEQUENCE {

 ue-Category-v11a0 INTEGER (11..12) OPTIONAL,

 measParameters-v11a0 MeasParameters-v11a0 OPTIONAL,

 nonCriticalExtension UE-EUTRA-Capability-v1250-IEs OPTIONAL

}

UE-EUTRA-Capability-v1250-IEs ::= SEQUENCE {

 phyLayerParameters-v1250 PhyLayerParameters-v1250 OPTIONAL,

 rf-Parameters-v1250 RF-Parameters-v1250 OPTIONAL,

 rlc-Parameters-r12 RLC-Parameters-r12 OPTIONAL,

 ue-BasedNetwPerfMeasParameters-v1250 UE-BasedNetwPerfMeasParameters-v1250 OPTIONAL,

 ue-CategoryDL-r12 INTEGER (0..14) OPTIONAL,

 ue-CategoryUL-r12 INTEGER (0..13) OPTIONAL,

 wlan-IW-Parameters-r12 WLAN-IW-Parameters-r12 OPTIONAL,

 measParameters-v1250 MeasParameters-v1250 OPTIONAL,

 dc-Parameters-r12 DC-Parameters-r12 OPTIONAL,

 mbms-Parameters-v1250 MBMS-Parameters-v1250 OPTIONAL,

 mac-Parameters-r12 MAC-Parameters-r12 OPTIONAL,

 fdd-Add-UE-EUTRA-Capabilities-v1250 UE-EUTRA-CapabilityAddXDD-Mode-v1250 OPTIONAL,

 tdd-Add-UE-EUTRA-Capabilities-v1250 UE-EUTRA-CapabilityAddXDD-Mode-v1250 OPTIONAL,

 sl-Parameters-r12 SL-Parameters-r12 OPTIONAL,

 nonCriticalExtension UE-EUTRA-Capability-v1260-IEs OPTIONAL

}

UE-EUTRA-Capability-v1260-IEs ::= SEQUENCE {

 ue-CategoryDL-v1260 INTEGER (15..16) OPTIONAL,

 nonCriticalExtension UE-EUTRA-Capability-v1270-IEs OPTIONAL

}

UE-EUTRA-Capability-v1270-IEs ::= SEQUENCE {

 rf-Parameters-v1270 RF-Parameters-v1270 OPTIONAL,

 nonCriticalExtension UE-EUTRA-Capability-v1280-IEs OPTIONAL

}

UE-EUTRA-Capability-v1280-IEs ::= SEQUENCE {

 phyLayerParameters-v1280 PhyLayerParameters-v1280 OPTIONAL,

 nonCriticalExtension UE-EUTRA-Capability-v1310-IEs OPTIONAL

}

UE-EUTRA-Capability-v1310-IEs ::= SEQUENCE {

 ue-CategoryDL-v1310 ENUMERATED {n17, m1} OPTIONAL,

 ue-CategoryUL-v1310 ENUMERATED {n14, m1} OPTIONAL,

 pdcp-Parameters-v1310 PDCP-Parameters-v1310,

 rlc-Parameters-v1310 RLC-Parameters-v1310,

 mac-Parameters-v1310 MAC-Parameters-v1310 OPTIONAL,

 phyLayerParameters-v1310 PhyLayerParameters-v1310 OPTIONAL,

 rf-Parameters-v1310 RF-Parameters-v1310 OPTIONAL,

 measParameters-v1310 MeasParameters-v1310 OPTIONAL,

 dc-Parameters-v1310 DC-Parameters-v1310 OPTIONAL,

 sl-Parameters-v1310 SL-Parameters-v1310 OPTIONAL,

 scptm-Parameters-r13 SCPTM-Parameters-r13 OPTIONAL,

 ce-Parameters-r13 CE-Parameters-r13 OPTIONAL,

 interRAT-ParametersWLAN-r13IRAT-ParametersWLAN-r13,

 laa-Parameters-r13 LAA-Parameters-r13 OPTIONAL,

 lwa-Parameters-r13 LWA-Parameters-r13 OPTIONAL,

 wlan-IW-Parameters-v1310 WLAN-IW-Parameters-v1310,

 lwip-Parameters-r13 LWIP-Parameters-r13,

 fdd-Add-UE-EUTRA-Capabilities-v1310 UE-EUTRA-CapabilityAddXDD-Mode-v1310 OPTIONAL,

 tdd-Add-UE-EUTRA-Capabilities-v1310 UE-EUTRA-CapabilityAddXDD-Mode-v1310 OPTIONAL,

 nonCriticalExtension UE-EUTRA-Capability-v1320-IEs OPTIONAL

}

UE-EUTRA-Capability-v1320-IEs ::= SEQUENCE {

 ce-Parameters-v1320 CE-Parameters-v1320 OPTIONAL,

 phyLayerParameters-v1320 PhyLayerParameters-v1320 OPTIONAL,

 rf-Parameters-v1320 RF-Parameters-v1320 OPTIONAL,

 fdd-Add-UE-EUTRA-Capabilities-v1320 UE-EUTRA-CapabilityAddXDD-Mode-v1320 OPTIONAL,

 tdd-Add-UE-EUTRA-Capabilities-v1320 UE-EUTRA-CapabilityAddXDD-Mode-v1320 OPTIONAL,

 nonCriticalExtension UE-EUTRA-Capability-v1330-IEs OPTIONAL

}

UE-EUTRA-Capability-v1330-IEs ::= SEQUENCE {

 ue-CategoryDL-v1330 INTEGER (18..19) OPTIONAL,

 phyLayerParameters-v1330 PhyLayerParameters-v1330 OPTIONAL,

 ue-CE-NeedULGaps-r13 ENUMERATED {true} OPTIONAL,

 nonCriticalExtension UE-EUTRA-Capability-v1340-IEs OPTIONAL

}

UE-EUTRA-Capability-v1340-IEs ::= SEQUENCE {

 ue-CategoryUL-v1340 INTEGER (15) OPTIONAL,

 nonCriticalExtension UE-EUTRA-Capability-v1350-IEs OPTIONAL

}

UE-EUTRA-Capability-v1350-IEs ::= SEQUENCE {

 ue-CategoryDL-v1350 ENUMERATED {oneBis} OPTIONAL,

 ue-CategoryUL-v1350 ENUMERATED {oneBis} OPTIONAL,

 ce-Parameters-v1350 CE-Parameters-v1350,

 nonCriticalExtension UE-EUTRA-Capability-v1360-IEs OPTIONAL

}

UE-EUTRA-Capability-v1360-IEs ::= SEQUENCE {

 other-Parameters-v1360 Other-Parameters-v1360 OPTIONAL,

 nonCriticalExtension UE-EUTRA-Capability-v1430-IEs OPTIONAL

}

UE-EUTRA-Capability-v1430-IEs ::= SEQUENCE {

 phyLayerParameters-v1430 PhyLayerParameters-v1430,

 ue-CategoryDL-v1430 ENUMERATED {m2} OPTIONAL,

 ue-CategoryUL-v1430 ENUMERATED {n16, n17, n18, n19, n20, m2} OPTIONAL,

 ue-CategoryUL-v1430b ENUMERATED {n21} OPTIONAL,

 mac-Parameters-v1430 MAC-Parameters-v1430 OPTIONAL,

 measParameters-v1430 MeasParameters-v1430 OPTIONAL,

 pdcp-Parameters-v1430 PDCP-Parameters-v1430 OPTIONAL,

 rlc-Parameters-v1430 RLC-Parameters-v1430,

 rf-Parameters-v1430 RF-Parameters-v1430 OPTIONAL,

 laa-Parameters-v1430 LAA-Parameters-v1430 OPTIONAL,

 lwa-Parameters-v1430 LWA-Parameters-v1430 OPTIONAL,

 lwip-Parameters-v1430 LWIP-Parameters-v1430 OPTIONAL,

 otherParameters-v1430 Other-Parameters-v1430,

 mmtel-Parameters-r14 MMTEL-Parameters-r14 OPTIONAL,

 mobilityParameters-r14 MobilityParameters-r14 OPTIONAL,

 ce-Parameters-v1430 CE-Parameters-v1430,

 fdd-Add-UE-EUTRA-Capabilities-v1430 UE-EUTRA-CapabilityAddXDD-Mode-v1430 OPTIONAL,

 tdd-Add-UE-EUTRA-Capabilities-v1430 UE-EUTRA-CapabilityAddXDD-Mode-v1430 OPTIONAL,

 mbms-Parameters-v1430 MBMS-Parameters-v1430 OPTIONAL,

 sl-Parameters-v1430 SL-Parameters-v1430 OPTIONAL,

 ue-BasedNetwPerfMeasParameters-v1430 UE-BasedNetwPerfMeasParameters-v1430 OPTIONAL,

 highSpeedEnhParameters-r14 HighSpeedEnhParameters-r14 OPTIONAL,

 nonCriticalExtension UE-EUTRA-Capability-v1440-IEs OPTIONAL

}

UE-EUTRA-Capability-v1440-IEs ::= SEQUENCE {

 lwa-Parameters-v1440 LWA-Parameters-v1440,

 mac-Parameters-v1440 MAC-Parameters-v1440,

 nonCriticalExtension UE-EUTRA-Capability-v1450-IEs OPTIONAL

}

UE-EUTRA-Capability-v1450-IEs ::= SEQUENCE {

 phyLayerParameters-v1450 PhyLayerParameters-v1450 OPTIONAL,

 rf-Parameters-v1450 RF-Parameters-v1450 OPTIONAL,

 otherParameters-v1450 OtherParameters-v1450,

 ue-CategoryDL-v1450 INTEGER (20) OPTIONAL,

 nonCriticalExtension UE-EUTRA-Capability-v1460-IEs OPTIONAL

}

UE-EUTRA-Capability-v1460-IEs ::= SEQUENCE {

 ue-CategoryDL-v1460 INTEGER (21) OPTIONAL,

 otherParameters-v1460 Other-Parameters-v1460,

 nonCriticalExtension UE-EUTRA-Capability-v1510-IEs OPTIONAL

}

UE-EUTRA-Capability-v1510-IEs ::= SEQUENCE {

 irat-ParametersNR-r15 IRAT-ParametersNR-r15 OPTIONAL,

 featureSetsEUTRA-r15 FeatureSetsEUTRA-r15 OPTIONAL,

 pdcp-ParametersNR-r15 PDCP-ParametersNR-r15 OPTIONAL,

 fdd-Add-UE-EUTRA-Capabilities-v1510 UE-EUTRA-CapabilityAddXDD-Mode-v1510 OPTIONAL,

 tdd-Add-UE-EUTRA-Capabilities-v1510 UE-EUTRA-CapabilityAddXDD-Mode-v1510 OPTIONAL,

 nonCriticalExtension UE-EUTRA-Capability-v1520-IEs OPTIONAL

}

UE-EUTRA-Capability-v1520-IEs ::= SEQUENCE {

 measParameters-v1520 MeasParameters-v1520,

 nonCriticalExtension UE-EUTRA-Capability-v1530-IEs OPTIONAL

}

UE-EUTRA-Capability-v1530-IEs ::= SEQUENCE {

 measParameters-v1530 MeasParameters-v1530 OPTIONAL,

 otherParameters-v1530 Other-Parameters-v1530 OPTIONAL,

 neighCellSI-AcquisitionParameters-v1530 NeighCellSI-AcquisitionParameters-v1530 OPTIONAL,

 mac-Parameters-v1530 MAC-Parameters-v1530 OPTIONAL,

 phyLayerParameters-v1530 PhyLayerParameters-v1530 OPTIONAL,

 rf-Parameters-v1530 RF-Parameters-v1530 OPTIONAL,

 pdcp-Parameters-v1530 PDCP-Parameters-v1530 OPTIONAL,

 ue-CategoryDL-v1530 INTEGER (22..26) OPTIONAL,

 ue-BasedNetwPerfMeasParameters-v1530 UE-BasedNetwPerfMeasParameters-v1530 OPTIONAL,

 rlc-Parameters-v1530 RLC-Parameters-v1530 OPTIONAL,

 sl-Parameters-v1530 SL-Parameters-v1530 OPTIONAL,

 extendedNumberOfDRBs-r15 ENUMERATED {supported} OPTIONAL,

 reducedCP-Latency-r15 ENUMERATED {supported} OPTIONAL,

 laa-Parameters-v1530 LAA-Parameters-v1530 OPTIONAL,

 ue-CategoryUL-v1530 INTEGER (22..26) OPTIONAL,

 fdd-Add-UE-EUTRA-Capabilities-v1530 UE-EUTRA-CapabilityAddXDD-Mode-v1530 OPTIONAL,

 tdd-Add-UE-EUTRA-Capabilities-v1530 UE-EUTRA-CapabilityAddXDD-Mode-v1530 OPTIONAL,

 nonCriticalExtension UE-EUTRA-Capability-v1540-IEs OPTIONAL

}

UE-EUTRA-Capability-v1540-IEs ::= SEQUENCE {

 phyLayerParameters-v1540 PhyLayerParameters-v1540 OPTIONAL,

 otherParameters-v1540 Other-Parameters-v1540,

 fdd-Add-UE-EUTRA-Capabilities-v1540 UE-EUTRA-CapabilityAddXDD-Mode-v1540 OPTIONAL,

 tdd-Add-UE-EUTRA-Capabilities-v1540 UE-EUTRA-CapabilityAddXDD-Mode-v1540 OPTIONAL,

 sl-Parameters-v1540 SL-Parameters-v1540 OPTIONAL,

 irat-ParametersNR-v1540 IRAT-ParametersNR-v1540 OPTIONAL,

 nonCriticalExtension UE-EUTRA-Capability-v1550-IEs OPTIONAL

}

UE-EUTRA-Capability-v1550-IEs ::= SEQUENCE {

 neighCellSI-AcquisitionParameters-v1550 NeighCellSI-AcquisitionParameters-v1550 OPTIONAL,

 phyLayerParameters-v1550 PhyLayerParameters-v1550,

 mac-Parameters-v1550 MAC-Parameters-v1550,

 fdd-Add-UE-EUTRA-Capabilities-v1550 UE-EUTRA-CapabilityAddXDD-Mode-v1550,

 tdd-Add-UE-EUTRA-Capabilities-v1550 UE-EUTRA-CapabilityAddXDD-Mode-v1550,

 nonCriticalExtension UE-EUTRA-Capability-v1560-IEs OPTIONAL

}

UE-EUTRA-Capability-v1560-IEs ::= SEQUENCE {

 pdcp-ParametersNR-v1560 PDCP-ParametersNR-v1560,

 irat-ParametersNR-v1560 IRAT-ParametersNR-v1560,

 appliedCapabilityFilterCommon-r15 OCTET STRING OPTIONAL,

 fdd-Add-UE-EUTRA-Capabilities-v1560 UE-EUTRA-CapabilityAddXDD-Mode-v1560,

 tdd-Add-UE-EUTRA-Capabilities-v1560 UE-EUTRA-CapabilityAddXDD-Mode-v1560,

 nonCriticalExtension UE-EUTRA-Capability-v1570-IEs OPTIONAL

}

UE-EUTRA-Capability-v1570-IEs ::= SEQUENCE {

 rf-Parameters-v1570 RF-Parameters-v1570 OPTIONAL,

 irat-ParametersNR-v1570 IRAT-ParametersNR-v1570 OPTIONAL,

 nonCriticalExtension UE-EUTRA-Capability-v15a0-IEs OPTIONAL

}

UE-EUTRA-Capability-v15a0-IEs ::= SEQUENCE {

 neighCellSI-AcquisitionParameters-v15a0 NeighCellSI-AcquisitionParameters-v15a0,

 eutra-5GC-Parameters-r15 EUTRA-5GC-Parameters-r15 OPTIONAL,

 fdd-Add-UE-EUTRA-Capabilities-v15a0 UE-EUTRA-CapabilityAddXDD-Mode-v15a0 OPTIONAL,

 tdd-Add-UE-EUTRA-Capabilities-v15a0 UE-EUTRA-CapabilityAddXDD-Mode-v15a0 OPTIONAL,

 nonCriticalExtension UE-EUTRA-Capability-v1610-IEs OPTIONAL

}

UE-EUTRA-Capability-v1610-IEs ::= SEQUENCE {

 highSpeedEnhParameters-v1610 HighSpeedEnhParameters-v1610 OPTIONAL,

 neighCellSI-AcquisitionParameters-v1610 NeighCellSI-AcquisitionParameters-v1610 OPTIONAL,

 mbms-Parameters-v1610 MBMS-Parameters-v1610 OPTIONAL,

 pdcp-Parameters-v1610 PDCP-Parameters-v1610 OPTIONAL,

 mac-Parameters-v1610 MAC-Parameters-v1610 OPTIONAL,

 phyLayerParameters-v1610 PhyLayerParameters-v1610 OPTIONAL,

 measParameters-v1610 MeasParameters-v1610 OPTIONAL,

 pur-Parameters-r16 PUR-Parameters-r16 OPTIONAL,

 eutra-5GC-Parameters-v1610 EUTRA-5GC-Parameters-v1610 OPTIONAL,

 otherParameters-v1610 Other-Parameters-v1610 OPTIONAL,

 dl-DedicatedMessageSegmentation-r16 ENUMERATED {supported} OPTIONAL,

 mmtel-Parameters-v1610 MMTEL-Parameters-v1610,

 irat-ParametersNR-v1610 IRAT-ParametersNR-v1610 OPTIONAL,

 rf-Parameters-v1610 RF-Parameters-v1610 OPTIONAL,

 mobilityParameters-v1610 MobilityParameters-v1610 OPTIONAL,

 ue-BasedNetwPerfMeasParameters-v1610 UE-BasedNetwPerfMeasParameters-v1610,

 sl-Parameters-v1610 SL-Parameters-v1610 OPTIONAL,

 fdd-Add-UE-EUTRA-Capabilities-v1610 UE-EUTRA-CapabilityAddXDD-Mode-v1610 OPTIONAL,

 tdd-Add-UE-EUTRA-Capabilities-v1610 UE-EUTRA-CapabilityAddXDD-Mode-v1610 OPTIONAL,

 nonCriticalExtension UE-EUTRA-Capability-v1630-IEs OPTIONAL

}

UE-EUTRA-Capability-v1630-IEs ::= SEQUENCE {

 rf-Parameters-v1630 RF-Parameters-v1630 OPTIONAL,

 sl-Parameters-v1630 SL-Parameters-v1630 OPTIONAL,

 earlySecurityReactivation-r16 ENUMERATED {supported} OPTIONAL,

 mac-Parameters-v1630 MAC-Parameters-v1630,

 measParameters-v1630 MeasParameters-v1630 OPTIONAL,

 fdd-Add-UE-EUTRA-Capabilities-v1630 UE-EUTRA-CapabilityAddXDD-Mode-v1630,

 tdd-Add-UE-EUTRA-Capabilities-v1630 UE-EUTRA-CapabilityAddXDD-Mode-v1630,

 nonCriticalExtension UE-EUTRA-Capability-v1650-IEs OPTIONAL

}

UE-EUTRA-Capability-v1650-IEs ::= SEQUENCE {

 otherParameters-v1650 Other-Parameters-v1650 OPTIONAL,

 nonCriticalExtension UE-EUTRA-Capability-v1660-IEs OPTIONAL

}

UE-EUTRA-Capability-v1660-IEs ::= SEQUENCE {

 irat-ParametersNR-v1660 IRAT-ParametersNR-v1660,

 nonCriticalExtension UE-EUTRA-Capability-v1690-IEs OPTIONAL

}

UE-EUTRA-Capability-v1690-IEs ::= SEQUENCE {

 other-Parameters-v1690 Other-Parameters-v1690,

 nonCriticalExtension UE-EUTRA-Capability-v1700-IEs OPTIONAL

}

UE-EUTRA-Capability-v1700-IEs ::= SEQUENCE {

 measParameters-v1700 MeasParameters-v1700 OPTIONAL,

 ue-BasedNetwPerfMeasParameters-v1700 UE-BasedNetwPerfMeasParameters-v1700 OPTIONAL,

 phyLayerParameters-v1700 PhyLayerParameters-v1700,

 ntn-Parameters-r17 NTN-Parameters-r17 OPTIONAL,

 irat-ParametersNR-v1700 IRAT-ParametersNR-v1700 OPTIONAL,

 mbms-Parameters-v1700 MBMS-Parameters-v1700,

 nonCriticalExtension UE-EUTRA-Capability-v1710-IEs OPTIONAL

}

UE-EUTRA-Capability-v1710-IEs ::= SEQUENCE {

 irat-ParametersNR-v1710 IRAT-ParametersNR-v1710,

 neighCellSI-AcquisitionParameters-v1710 NeighCellSI-AcquisitionParameters-v1710 OPTIONAL,

 sl-Parameters-v1710 SL-Parameters-v1710 OPTIONAL,

 sidelinkRequested-r17 ENUMERATED {true} OPTIONAL,

 nonCriticalExtension UE-EUTRA-Capability-v1720-IEs OPTIONAL

}

UE-EUTRA-Capability-v1720-IEs ::= SEQUENCE {

 ntn-Parameters-v1720 NTN-Parameters-v1720,

 nonCriticalExtension UE-EUTRA-Capability-v1730-IEs OPTIONAL

}

UE-EUTRA-Capability-v1730-IEs ::= SEQUENCE {

 phyLayerParameters-v1730 PhyLayerParameters-v1730,

 nonCriticalExtension UE-EUTRA-Capability-v1770-IEs OPTIONAL

}

UE-EUTRA-Capability-v1770-IEs ::= SEQUENCE {

 measParameters-v1770 MeasParameters-v1770,

 nonCriticalExtension UE-EUTRA-Capability-v1800-IEs OPTIONAL

}

UE-EUTRA-Capability-v1800-IEs ::= SEQUENCE {

 measParameters-v1800 MeasParameters-v1800 OPTIONAL,

 rf-Parameters-v1800 RF-Parameters-v1800 OPTIONAL,

 ntn-Parameters-v1800 NTN-Parameters-v1800 OPTIONAL,

 -- A2X capabilities

 sl-Parameters-v1800 SL-Parameters-v1800 OPTIONAL,

 son-Parameters-v1800 SON-Parameters-v1800,

 ue-BasedNetwPerfMeasParameters-v1800 UE-BasedNetwPerfMeasParameters-v1800,

 nonCriticalExtension UE-EUTRA-Capability-v1830-IEs OPTIONAL

}

UE-EUTRA-Capability-v1830-IEs ::= SEQUENCE {

 ntn-Parameters-v1830 NTN-Parameters-v1830,

 nonCriticalExtension UE-EUTRA-Capability-v1840-IEs OPTIONAL

}

UE-EUTRA-Capability-v1840-IEs ::= SEQUENCE {

 measParameters-v1840 MeasParameters-v1840,

 nonCriticalExtension UE-EUTRA-Capability-v19xy-IEs OPTIONAL

}

UE-EUTRA-Capability-v19xy-IEs ::= SEQUENCE {

 irat-ParametersNR-v19xy IRAT-ParametersNR-v19xy,

 nonCriticalExtension SEQUENCE {} OPTIONAL

}

UE-EUTRA-CapabilityAddXDD-Mode-r9 ::= SEQUENCE {

 phyLayerParameters-r9 PhyLayerParameters OPTIONAL,

 featureGroupIndicators-r9 BIT STRING (SIZE (32)) OPTIONAL,

 featureGroupIndRel9Add-r9 BIT STRING (SIZE (32)) OPTIONAL,

 interRAT-ParametersGERAN-r9 IRAT-ParametersGERAN OPTIONAL,

 interRAT-ParametersUTRA-r9 IRAT-ParametersUTRA-v920 OPTIONAL,

 interRAT-ParametersCDMA2000-r9 IRAT-ParametersCDMA2000-1XRTT-v920 OPTIONAL,

 neighCellSI-AcquisitionParameters-r9 NeighCellSI-AcquisitionParameters-r9 OPTIONAL,

 ...

}

UE-EUTRA-CapabilityAddXDD-Mode-v1060 ::= SEQUENCE {

 phyLayerParameters-v1060 PhyLayerParameters-v1020 OPTIONAL,

 featureGroupIndRel10-v1060 BIT STRING (SIZE (32)) OPTIONAL,

 interRAT-ParametersCDMA2000-v1060 IRAT-ParametersCDMA2000-1XRTT-v1020 OPTIONAL,

 interRAT-ParametersUTRA-TDD-v1060 IRAT-ParametersUTRA-TDD-v1020 OPTIONAL,

 ...,

 [[ otdoa-PositioningCapabilities-r10 OTDOA-PositioningCapabilities-r10 OPTIONAL

 ]]

}

UE-EUTRA-CapabilityAddXDD-Mode-v1130 ::= SEQUENCE {

 phyLayerParameters-v1130 PhyLayerParameters-v1130 OPTIONAL,

 measParameters-v1130 MeasParameters-v1130 OPTIONAL,

 otherParameters-r11 Other-Parameters-r11 OPTIONAL,

 ...

}

UE-EUTRA-CapabilityAddXDD-Mode-v1180 ::= SEQUENCE {

 mbms-Parameters-r11 MBMS-Parameters-r11

}

UE-EUTRA-CapabilityAddXDD-Mode-v1250 ::= SEQUENCE {

 phyLayerParameters-v1250 PhyLayerParameters-v1250 OPTIONAL,

 measParameters-v1250 MeasParameters-v1250 OPTIONAL

}

UE-EUTRA-CapabilityAddXDD-Mode-v1310 ::= SEQUENCE {

 phyLayerParameters-v1310 PhyLayerParameters-v1310 OPTIONAL

}

UE-EUTRA-CapabilityAddXDD-Mode-v1320 ::= SEQUENCE {

 phyLayerParameters-v1320 PhyLayerParameters-v1320 OPTIONAL,

 scptm-Parameters-r13 SCPTM-Parameters-r13 OPTIONAL

}

UE-EUTRA-CapabilityAddXDD-Mode-v1370 ::= SEQUENCE {

 ce-Parameters-v1370 CE-Parameters-v1370 OPTIONAL

}

UE-EUTRA-CapabilityAddXDD-Mode-v1380 ::= SEQUENCE {

 ce-Parameters-v1380 CE-Parameters-v1380

}

UE-EUTRA-CapabilityAddXDD-Mode-v1430 ::= SEQUENCE {

 phyLayerParameters-v1430 PhyLayerParameters-v1430 OPTIONAL,

 mmtel-Parameters-r14 MMTEL-Parameters-r14 OPTIONAL

}

UE-EUTRA-CapabilityAddXDD-Mode-v1510 ::= SEQUENCE {

 pdcp-ParametersNR-r15 PDCP-ParametersNR-r15 OPTIONAL

}

UE-EUTRA-CapabilityAddXDD-Mode-v1530 ::= SEQUENCE {

 neighCellSI-AcquisitionParameters-v1530 NeighCellSI-AcquisitionParameters-v1530 OPTIONAL,

 reducedCP-Latency-r15 ENUMERATED {supported} OPTIONAL

}

UE-EUTRA-CapabilityAddXDD-Mode-v1540 ::= SEQUENCE {

 eutra-5GC-Parameters-r15 EUTRA-5GC-Parameters-r15 OPTIONAL,

 irat-ParametersNR-v1540 IRAT-ParametersNR-v1540 OPTIONAL

}

UE-EUTRA-CapabilityAddXDD-Mode-v1550 ::= SEQUENCE {

 neighCellSI-AcquisitionParameters-v1550 NeighCellSI-AcquisitionParameters-v1550 OPTIONAL

}

UE-EUTRA-CapabilityAddXDD-Mode-v1560 ::= SEQUENCE {

 pdcp-ParametersNR-v1560 PDCP-ParametersNR-v1560

}

UE-EUTRA-CapabilityAddXDD-Mode-v15a0 ::= SEQUENCE {

 phyLayerParameters-v1530 PhyLayerParameters-v1530 OPTIONAL,

 phyLayerParameters-v1540 PhyLayerParameters-v1540 OPTIONAL,

 phyLayerParameters-v1550 PhyLayerParameters-v1550 OPTIONAL,

 neighCellSI-AcquisitionParameters-v15a0 NeighCellSI-AcquisitionParameters-v15a0

}

UE-EUTRA-CapabilityAddXDD-Mode-v1610 ::= SEQUENCE {

 phyLayerParameters-v1610 PhyLayerParameters-v1610 OPTIONAL,

 pur-Parameters-r16 PUR-Parameters-r16 OPTIONAL,

 measParameters-v1610 MeasParameters-v1610 OPTIONAL,

 eutra-5GC-Parameters-v1610 EUTRA-5GC-Parameters-v1610 OPTIONAL,

 irat-ParametersNR-v1610 IRAT-ParametersNR-v1610 OPTIONAL,

 neighCellSI-AcquisitionParameters-v1610 NeighCellSI-AcquisitionParameters-v1610 OPTIONAL,

 mobilityParameters-v1610 MobilityParameters-v1610 OPTIONAL

}

UE-EUTRA-CapabilityAddXDD-Mode-v1630 ::= SEQUENCE {

 measParameters-v1630 MeasParameters-v1630

}

AccessStratumRelease ::= ENUMERATED {

 rel8, rel9, rel10, rel11, rel12, rel13,

 rel14, rel15, ..., rel16, rel17, rel18}

FeatureSetsEUTRA-r15 ::= SEQUENCE {

 featureSetsDL-r15 SEQUENCE (SIZE (1..maxFeatureSets-r15)) OF FeatureSetDL-r15 OPTIONAL,

 featureSetsDL-PerCC-r15 SEQUENCE (SIZE (1..maxPerCC-FeatureSets-r15)) OF FeatureSetDL-PerCC-r15 OPTIONAL,

 featureSetsUL-r15 SEQUENCE (SIZE (1..maxFeatureSets-r15)) OF FeatureSetUL-r15 OPTIONAL,

 featureSetsUL-PerCC-r15 SEQUENCE (SIZE (1..maxPerCC-FeatureSets-r15)) OF FeatureSetUL-PerCC-r15 OPTIONAL,

 ...,

 [[ featureSetsDL-v1550 SEQUENCE (SIZE (1..maxFeatureSets-r15)) OF FeatureSetDL-v1550 OPTIONAL

 ]]

}

MobilityParameters-r14 ::= SEQUENCE {

 makeBeforeBreak-r14 ENUMERATED {supported} OPTIONAL,

 rach-Less-r14 ENUMERATED {supported} OPTIONAL

}

MobilityParameters-v1610 ::= SEQUENCE {

 cho-r16 ENUMERATED {supported} OPTIONAL,

 cho-FDD-TDD-r16 ENUMERATED {supported} OPTIONAL,

 cho-Failure-r16 ENUMERATED {supported} OPTIONAL,

 cho-TwoTriggerEvents-r16 ENUMERATED {supported} OPTIONAL

}

DC-Parameters-r12 ::= SEQUENCE {

 drb-TypeSplit-r12 ENUMERATED {supported} OPTIONAL,

 drb-TypeSCG-r12 ENUMERATED {supported} OPTIONAL

}

DC-Parameters-v1310 ::= SEQUENCE {

 pdcp-TransferSplitUL-r13 ENUMERATED {supported} OPTIONAL,

 ue-SSTD-Meas-r13 ENUMERATED {supported} OPTIONAL

}

MAC-Parameters-r12 ::= SEQUENCE {

 logicalChannelSR-ProhibitTimer-r12 ENUMERATED {supported} OPTIONAL,

 longDRX-Command-r12 ENUMERATED {supported} OPTIONAL

}

MAC-Parameters-v1310 ::= SEQUENCE {

 extendedMAC-LengthField-r13 ENUMERATED {supported} OPTIONAL,

 extendedLongDRX-r13 ENUMERATED {supported} OPTIONAL

}

MAC-Parameters-v1430 ::= SEQUENCE {

 shortSPS-IntervalFDD-r14 ENUMERATED {supported} OPTIONAL,

 shortSPS-IntervalTDD-r14 ENUMERATED {supported} OPTIONAL,

 skipUplinkDynamic-r14 ENUMERATED {supported} OPTIONAL,

 skipUplinkSPS-r14 ENUMERATED {supported} OPTIONAL,

 multipleUplinkSPS-r14 ENUMERATED {supported} OPTIONAL,

 dataInactMon-r14 ENUMERATED {supported} OPTIONAL

}

MAC-Parameters-v1440 ::= SEQUENCE {

 rai-Support-r14 ENUMERATED {supported} OPTIONAL

}

MAC-Parameters-v1530 ::= SEQUENCE {

 min-Proc-TimelineSubslot-r15 SEQUENCE (SIZE(1..3)) OF ProcessingTimelineSet-r15 OPTIONAL,

 skipSubframeProcessing-r15 SkipSubframeProcessing-r15 OPTIONAL,

 earlyData-UP-r15 ENUMERATED {supported} OPTIONAL,

 dormantSCellState-r15 ENUMERATED {supported} OPTIONAL,

 directSCellActivation-r15 ENUMERATED {supported} OPTIONAL,

 directSCellHibernation-r15 ENUMERATED {supported} OPTIONAL,

 extendedLCID-Duplication-r15 ENUMERATED {supported} OPTIONAL,

 sps-ServingCell-r15 ENUMERATED {supported} OPTIONAL

}

MAC-Parameters-v1550 ::= SEQUENCE {

 eLCID-Support-r15 ENUMERATED {supported} OPTIONAL

}

MAC-Parameters-v1610 ::= SEQUENCE {

 directMCG-SCellActivationResume-r16 ENUMERATED {supported} OPTIONAL,

 directSCG-SCellActivationResume-r16 ENUMERATED {supported} OPTIONAL,

 earlyData-UP-5GC-r16 ENUMERATED {supported} OPTIONAL,

 rai-SupportEnh-r16 ENUMERATED {supported} OPTIONAL

}

MAC-Parameters-v1630 ::= SEQUENCE {

 directSCG-SCellActivationNEDC-r16 ENUMERATED {supported} OPTIONAL

}

NTN-Parameters-r17 ::= SEQUENCE {

 ntn-Connectivity-EPC-r17 ENUMERATED {supported} OPTIONAL,

 ntn-TA-Report-r17 ENUMERATED {supported} OPTIONAL,

 ntn-PUR-TimerDelay-r17 ENUMERATED {supported} OPTIONAL,

 ntn-OffsetTimingEnh-r17 ENUMERATED {supported} OPTIONAL,

 ntn-ScenarioSupport-r17 ENUMERATED {ngso,gso} OPTIONAL

}

NTN-Parameters-v1720 ::= SEQUENCE {

 ntn-SegmentedPrecompensationGaps-r17 ENUMERATED {sym1,sl1,sf1} OPTIONAL

}

NTN-Parameters-v1800 ::= SEQUENCE {

 ntn-EventA4BasedCHO-r18 ENUMERATED {supported} OPTIONAL,

 ntn-LocationBasedCHO-EFC-r18 ENUMERATED {supported} OPTIONAL,

 ntn-LocationBasedCHO-EMC-r18 ENUMERATED {supported} OPTIONAL,

 ntn-TimeBasedCHO-r18 ENUMERATED {supported} OPTIONAL,

 eventD1-MeasReportTrigger-r18 ENUMERATED {supported} OPTIONAL,

 eventD2-MeasReportTrigger-r18 ENUMERATED {supported} OPTIONAL,

 ntn-LocationBasedMeasTrigger-EFC-r18 ENUMERATED {supported} OPTIONAL,

 ntn-LocationBasedMeasTrigger-EMC-r18 ENUMERATED {supported} OPTIONAL,

 ntn-TimeBasedMeasTrigger-r18 ENUMERATED {supported} OPTIONAL,

 ntn-RRC-HarqDisableSingleTB-CE-ModeA-r18 ENUMERATED {supported} OPTIONAL,

 ntn-RRC-HarqDisableMultiTB-CE-ModeA-r18 ENUMERATED {supported} OPTIONAL,

 ntn-RRC-HarqDisableSingleTB-CE-ModeB-r18 ENUMERATED {supported} OPTIONAL,

 ntn-OverriddenHarqDisableSingleTB-CE-ModeB-r18 ENUMERATED {supported} OPTIONAL,

 ntn-DCI-HarqDisableSingleTB-CE-ModeB-r18 ENUMERATED {supported} OPTIONAL,

 ntn-RRC-HarqDisableMultiTB-CE-ModeB-r18 ENUMERATED {supported} OPTIONAL,

 ntn-OverriddenHarqDisableMultiTB-CE-ModeB-r18 ENUMERATED {supported} OPTIONAL,

 ntn-DCI-HarqDisableMultiTB-CE-ModeB-r18 ENUMERATED {supported} OPTIONAL,

 ntn-SemiStaticHarqDisableSPS-r18 ENUMERATED {supported} OPTIONAL,

 ntn-UplinkHarq-ModeB-SingleTB-r18 ENUMERATED {supported} OPTIONAL,

 ntn-UplinkHarq-ModeB-MultiTB-r18 ENUMERATED {supported} OPTIONAL,

 ntn-HarqEnhScenarioSupport-r18 ENUMERATED {ngso,gso} OPTIONAL,

 ntn-Triggered-GNSS-Fix-r18 ENUMERATED {supported} OPTIONAL,

 ntn-Autonomous-GNSS-Fix-r18 ENUMERATED {supported} OPTIONAL,

 ntn-UplinkTxExtension-r18 ENUMERATED {supported} OPTIONAL,

 ntn-GNSS-EnhScenarioSupport-r18 ENUMERATED {ngso,gso} OPTIONAL

}

NTN-Parameters-v1830 ::= SEQUENCE {

 satelliteInfoConfigDedicated-r18 ENUMERATED {supported} OPTIONAL

}

ProcessingTimelineSet-r15 ::= ENUMERATED {set1, set2}

RLC-Parameters-r12 ::= SEQUENCE {

 extended-RLC-LI-Field-r12 ENUMERATED {supported}

}

RLC-Parameters-v1310 ::= SEQUENCE {

 extendedRLC-SN-SO-Field-r13 ENUMERATED {supported} OPTIONAL

}

RLC-Parameters-v1430 ::= SEQUENCE {

 extendedPollByte-r14 ENUMERATED {supported} OPTIONAL

}

RLC-Parameters-v1530 ::= SEQUENCE {

 flexibleUM-AM-Combinations-r15 ENUMERATED {supported} OPTIONAL,

 rlc-AM-Ooo-Delivery-r15 ENUMERATED {supported} OPTIONAL,

 rlc-UM-Ooo-Delivery-r15 ENUMERATED {supported} OPTIONAL

}

PDCP-Parameters ::= SEQUENCE {

 supportedROHC-Profiles ROHC-ProfileSupportList-r15,

 maxNumberROHC-ContextSessions ENUMERATED {

 cs2, cs4, cs8, cs12, cs16, cs24, cs32,

 cs48, cs64, cs128, cs256, cs512, cs1024,

 cs16384, spare2, spare1} DEFAULT cs16,

 ...

}

PDCP-Parameters-v1130 ::= SEQUENCE {

 pdcp-SN-Extension-r11 ENUMERATED {supported} OPTIONAL,

 supportRohcContextContinue-r11 ENUMERATED {supported} OPTIONAL

}

PDCP-Parameters-v1310 ::= SEQUENCE {

 pdcp-SN-Extension-18bits-r13 ENUMERATED {supported} OPTIONAL

}

PDCP-Parameters-v1430 ::= SEQUENCE {

 supportedUplinkOnlyROHC-Profiles-r14 SEQUENCE {

 profile0x0006-r14 BOOLEAN

 },

 maxNumberROHC-ContextSessions-r14 ENUMERATED {

 cs2, cs4, cs8, cs12, cs16, cs24, cs32,

 cs48, cs64, cs128, cs256, cs512, cs1024,

 cs16384, spare2, spare1} DEFAULT cs16

}

PDCP-Parameters-v1530 ::= SEQUENCE {

 supportedUDC-r15 SupportedUDC-r15 OPTIONAL,

 pdcp-Duplication-r15 ENUMERATED {supported} OPTIONAL

}

PDCP-Parameters-v1610 ::= SEQUENCE {

 pdcp-VersionChangeWithoutHO-r16 ENUMERATED {supported} OPTIONAL,

 ehc-r16 ENUMERATED {supported} OPTIONAL,

 continueEHC-Context-r16 ENUMERATED {supported} OPTIONAL,

 maxNumberEHC-Contexts-r16 ENUMERATED {cs2, cs4, cs8, cs16, cs32, cs64, cs128, cs256,

 cs512, cs1024, cs2048, cs4096, cs8192, cs16384,

 cs32768, cs65536} OPTIONAL,

 jointEHC-ROHC-Config-r16 ENUMERATED {supported} OPTIONAL

}

SupportedUDC-r15 ::= SEQUENCE {

 supportedStandardDic-r15 ENUMERATED {supported} OPTIONAL,

 supportedOperatorDic-r15 SupportedOperatorDic-r15 OPTIONAL

}

SupportedOperatorDic-r15 ::= SEQUENCE {

 versionOfDictionary-r15 INTEGER (0..15),

 associatedPLMN-ID-r15 PLMN-Identity

}

PhyLayerParameters ::= SEQUENCE {

 ue-TxAntennaSelectionSupported BOOLEAN,

 ue-SpecificRefSigsSupported BOOLEAN

}

PhyLayerParameters-v920 ::= SEQUENCE {

 enhancedDualLayerFDD-r9 ENUMERATED {supported} OPTIONAL,

 enhancedDualLayerTDD-r9 ENUMERATED {supported} OPTIONAL

}

PhyLayerParameters-v9d0 ::= SEQUENCE {

 tm5-FDD-r9 ENUMERATED {supported} OPTIONAL,

 tm5-TDD-r9 ENUMERATED {supported} OPTIONAL

}

PhyLayerParameters-v1020 ::= SEQUENCE {

 twoAntennaPortsForPUCCH-r10 ENUMERATED {supported} OPTIONAL,

 tm9-With-8Tx-FDD-r10 ENUMERATED {supported} OPTIONAL,

 pmi-Disabling-r10 ENUMERATED {supported} OPTIONAL,

 crossCarrierScheduling-r10 ENUMERATED {supported} OPTIONAL,

 simultaneousPUCCH-PUSCH-r10 ENUMERATED {supported} OPTIONAL,

 multiClusterPUSCH-WithinCC-r10 ENUMERATED {supported} OPTIONAL,

 nonContiguousUL-RA-WithinCC-List-r10 NonContiguousUL-RA-WithinCC-List-r10 OPTIONAL

}

PhyLayerParameters-v1130 ::= SEQUENCE {

 crs-InterfHandl-r11 ENUMERATED {supported} OPTIONAL,

 ePDCCH-r11 ENUMERATED {supported} OPTIONAL,

 multiACK-CSI-Reporting-r11 ENUMERATED {supported} OPTIONAL,

 ss-CCH-InterfHandl-r11 ENUMERATED {supported} OPTIONAL,

 tdd-SpecialSubframe-r11 ENUMERATED {supported} OPTIONAL,

 txDiv-PUCCH1b-ChSelect-r11 ENUMERATED {supported} OPTIONAL,

 ul-CoMP-r11 ENUMERATED {supported} OPTIONAL

}

PhyLayerParameters-v1170 ::= SEQUENCE {

 interBandTDD-CA-WithDifferentConfig-r11 BIT STRING (SIZE (2)) OPTIONAL

}

PhyLayerParameters-v1250 ::= SEQUENCE {

 e-HARQ-Pattern-FDD-r12 ENUMERATED {supported} OPTIONAL,

 enhanced-4TxCodebook-r12 ENUMERATED {supported} OPTIONAL,

 tdd-FDD-CA-PCellDuplex-r12 BIT STRING (SIZE (2)) OPTIONAL,

 phy-TDD-ReConfig-TDD-PCell-r12 ENUMERATED {supported} OPTIONAL,

 phy-TDD-ReConfig-FDD-PCell-r12 ENUMERATED {supported} OPTIONAL,

 pusch-FeedbackMode-r12 ENUMERATED {supported} OPTIONAL,

 pusch-SRS-PowerControl-SubframeSet-r12 ENUMERATED {supported} OPTIONAL,

 csi-SubframeSet-r12 ENUMERATED {supported} OPTIONAL,

 noResourceRestrictionForTTIBundling-r12 ENUMERATED {supported} OPTIONAL,

 discoverySignalsInDeactSCell-r12 ENUMERATED {supported} OPTIONAL,

 naics-Capability-List-r12 NAICS-Capability-List-r12 OPTIONAL

}

PhyLayerParameters-v1280 ::= SEQUENCE {

 alternativeTBS-Indices-r12 ENUMERATED {supported} OPTIONAL

}

PhyLayerParameters-v1310 ::= SEQUENCE {

 aperiodicCSI-Reporting-r13 BIT STRING (SIZE (2)) OPTIONAL,

 codebook-HARQ-ACK-r13 BIT STRING (SIZE (2)) OPTIONAL,

 crossCarrierScheduling-B5C-r13 ENUMERATED {supported} OPTIONAL,

 fdd-HARQ-TimingTDD-r13 ENUMERATED {supported} OPTIONAL,

 maxNumberUpdatedCSI-Proc-r13 INTEGER(5..32) OPTIONAL,

 pucch-Format4-r13 ENUMERATED {supported} OPTIONAL,

 pucch-Format5-r13 ENUMERATED {supported} OPTIONAL,

 pucch-SCell-r13 ENUMERATED {supported} OPTIONAL,

 spatialBundling-HARQ-ACK-r13 ENUMERATED {supported} OPTIONAL,

 supportedBlindDecoding-r13 SEQUENCE {

 maxNumberDecoding-r13 INTEGER(1..32) OPTIONAL,

 pdcch-CandidateReductions-r13 ENUMERATED {supported} OPTIONAL,

 skipMonitoringDCI-Format0-1A-r13 ENUMERATED {supported} OPTIONAL

 } OPTIONAL,

 uci-PUSCH-Ext-r13 ENUMERATED {supported} OPTIONAL,

 crs-InterfMitigationTM10-r13 ENUMERATED {supported} OPTIONAL,

 pdsch-CollisionHandling-r13 ENUMERATED {supported} OPTIONAL

}

PhyLayerParameters-v1320 ::= SEQUENCE {

 mimo-UE-Parameters-r13 MIMO-UE-Parameters-r13 OPTIONAL

}

PhyLayerParameters-v1330 ::= SEQUENCE {

 cch-InterfMitigation-RefRecTypeA-r13 ENUMERATED {supported} OPTIONAL,

 cch-InterfMitigation-RefRecTypeB-r13 ENUMERATED {supported} OPTIONAL,

 cch-InterfMitigation-MaxNumCCs-r13 INTEGER (1.. maxServCell-r13) OPTIONAL,

 crs-InterfMitigationTM1toTM9-r13 INTEGER (1.. maxServCell-r13) OPTIONAL

}

PhyLayerParameters-v13e0 ::= SEQUENCE {

 mimo-UE-Parameters-v13e0 MIMO-UE-Parameters-v13e0

}

PhyLayerParameters-v1430 ::= SEQUENCE {

 ce-PUSCH-NB-MaxTBS-r14 ENUMERATED {supported} OPTIONAL,

 ce-PDSCH-PUSCH-MaxBandwidth-r14 ENUMERATED {bw5, bw20} OPTIONAL,

 ce-HARQ-AckBundling-r14 ENUMERATED {supported} OPTIONAL,

 ce-PDSCH-TenProcesses-r14 ENUMERATED {supported} OPTIONAL,

 ce-RetuningSymbols-r14 ENUMERATED {n0, n1} OPTIONAL,

 ce-PDSCH-PUSCH-Enhancement-r14 ENUMERATED {supported} OPTIONAL,

 ce-SchedulingEnhancement-r14 ENUMERATED {supported} OPTIONAL,

 ce-SRS-Enhancement-r14 ENUMERATED {supported} OPTIONAL,

 ce-PUCCH-Enhancement-r14 ENUMERATED {supported} OPTIONAL,

 ce-ClosedLoopTxAntennaSelection-r14 ENUMERATED {supported} OPTIONAL,

 tdd-SpecialSubframe-r14 ENUMERATED {supported} OPTIONAL,

 tdd-TTI-Bundling-r14 ENUMERATED {supported} OPTIONAL,

 dmrs-LessUpPTS-r14 ENUMERATED {supported} OPTIONAL,

 mimo-UE-Parameters-v1430 MIMO-UE-Parameters-v1430 OPTIONAL,

 alternativeTBS-Index-r14 ENUMERATED {supported} OPTIONAL,

 feMBMS-Unicast-Parameters-r14 FeMBMS-Unicast-Parameters-r14 OPTIONAL

}

PhyLayerParameters-v1450 ::= SEQUENCE {

 ce-SRS-EnhancementWithoutComb4-r14 ENUMERATED {supported} OPTIONAL,

 crs-LessDwPTS-r14 ENUMERATED {supported} OPTIONAL}

PhyLayerParameters-v1470 ::= SEQUENCE {

 mimo-UE-Parameters-v1470 MIMO-UE-Parameters-v1470 OPTIONAL,

 srs-UpPTS-6sym-r14 ENUMERATED {supported} OPTIONAL

}

PhyLayerParameters-v14a0 ::= SEQUENCE {

 ssp10-TDD-Only-r14 ENUMERATED {supported} OPTIONAL

}

PhyLayerParameters-v1530 ::= SEQUENCE {

 stti-SPT-Capabilities-r15 SEQUENCE {

 aperiodicCsi-ReportingSTTI-r15 ENUMERATED {supported} OPTIONAL,

 dmrs-BasedSPDCCH-MBSFN-r15 ENUMERATED {supported} OPTIONAL,

 dmrs-BasedSPDCCH-nonMBSFN-r15 ENUMERATED {supported} OPTIONAL,

 dmrs-PositionPattern-r15 ENUMERATED {supported} OPTIONAL,

 dmrs-SharingSubslotPDSCH-r15 ENUMERATED {supported} OPTIONAL,

 dmrs-RepetitionSubslotPDSCH-r15 ENUMERATED {supported} OPTIONAL,

 epdcch-SPT-differentCells-r15 ENUMERATED {supported} OPTIONAL,

 epdcch-STTI-differentCells-r15 ENUMERATED {supported} OPTIONAL,

 maxLayersSlotOrSubslotPUSCH-r15 ENUMERATED {oneLayer,twoLayers,fourLayers}

 OPTIONAL,

 maxNumberUpdatedCSI-Proc-SPT-r15 INTEGER(5..32) OPTIONAL,

 maxNumberUpdatedCSI-Proc-STTI-Comb77-r15 INTEGER(1..32) OPTIONAL,

 maxNumberUpdatedCSI-Proc-STTI-Comb27-r15 INTEGER(1..32) OPTIONAL,

 maxNumberUpdatedCSI-Proc-STTI-Comb22-Set1-r15 INTEGER(1..32) OPTIONAL,

 maxNumberUpdatedCSI-Proc-STTI-Comb22-Set2-r15 INTEGER(1..32) OPTIONAL,

 mimo-UE-ParametersSTTI-r15 MIMO-UE-Parameters-r13 OPTIONAL,

 mimo-UE-ParametersSTTI-v1530 MIMO-UE-Parameters-v1430 OPTIONAL,

 numberOfBlindDecodesUSS-r15 INTEGER(4..32) OPTIONAL,

 pdsch-SlotSubslotPDSCH-Decoding-r15 ENUMERATED {supported} OPTIONAL,

 powerUCI-SlotPUSCH ENUMERATED {supported} OPTIONAL,

 powerUCI-SubslotPUSCH ENUMERATED {supported} OPTIONAL,

 slotPDSCH-TxDiv-TM9and10 ENUMERATED {supported} OPTIONAL,

 subslotPDSCH-TxDiv-TM9and10 ENUMERATED {supported} OPTIONAL,

 spdcch-differentRS-types-r15 ENUMERATED {supported} OPTIONAL,

 srs-DCI7-TriggeringFS2-r15 ENUMERATED {supported} OPTIONAL,

 sps-cyclicShift-r15 ENUMERATED {supported} OPTIONAL,

 spdcch-Reuse-r15 ENUMERATED {supported} OPTIONAL,

 sps-STTI-r15 ENUMERATED {slot, subslot, slotAndSubslot}

 OPTIONAL,

 tm8-slotPDSCH-r15 ENUMERATED {supported} OPTIONAL,

 tm9-slotSubslot-r15 ENUMERATED {supported} OPTIONAL,

 tm9-slotSubslotMBSFN-r15 ENUMERATED {supported} OPTIONAL,

 tm10-slotSubslot-r15 ENUMERATED {supported} OPTIONAL,

 tm10-slotSubslotMBSFN-r15 ENUMERATED {supported} OPTIONAL,

 txDiv-SPUCCH-r15 ENUMERATED {supported} OPTIONAL,

 ul-AsyncHarqSharingDiff-TTI-Lengths-r15 ENUMERATED {supported} OPTIONAL

 } OPTIONAL,

 ce-Capabilities-r15 SEQUENCE {

 ce-CRS-IntfMitig-r15 ENUMERATED {supported} OPTIONAL,

 ce-CQI-AlternativeTable-r15 ENUMERATED {supported} OPTIONAL,

 ce-PDSCH-FlexibleStartPRB-CE-ModeA-r15 ENUMERATED {supported} OPTIONAL,

 ce-PDSCH-FlexibleStartPRB-CE-ModeB-r15 ENUMERATED {supported} OPTIONAL,

 ce-PDSCH-64QAM-r15 ENUMERATED {supported} OPTIONAL,

 ce-PUSCH-FlexibleStartPRB-CE-ModeA-r15 ENUMERATED {supported} OPTIONAL,

 ce-PUSCH-FlexibleStartPRB-CE-ModeB-r15 ENUMERATED {supported} OPTIONAL,

 ce-PUSCH-SubPRB-Allocation-r15 ENUMERATED {supported} OPTIONAL,

 ce-UL-HARQ-ACK-Feedback-r15 ENUMERATED {supported} OPTIONAL

 } OPTIONAL,

 shortCQI-ForSCellActivation-r15 ENUMERATED {supported} OPTIONAL,

 mimo-CBSR-AdvancedCSI-r15 ENUMERATED {supported} OPTIONAL,

 crs-IntfMitig-r15 ENUMERATED {supported} OPTIONAL,

 ul-PowerControlEnhancements-r15 ENUMERATED {supported} OPTIONAL,

 urllc-Capabilities-r15 SEQUENCE {

 pdsch-RepSubframe-r15 ENUMERATED {supported} OPTIONAL,

 pdsch-RepSlot-r15 ENUMERATED {supported} OPTIONAL,

 pdsch-RepSubslot-r15 ENUMERATED {supported} OPTIONAL,

 pusch-SPS-MultiConfigSubframe-r15 INTEGER (0..6) OPTIONAL,

 pusch-SPS-MaxConfigSubframe-r15 INTEGER (0..31) OPTIONAL,

 pusch-SPS-MultiConfigSlot-r15 INTEGER (0..6) OPTIONAL,

 pusch-SPS-MaxConfigSlot-r15 INTEGER (0..31) OPTIONAL,

 pusch-SPS-MultiConfigSubslot-r15 INTEGER (0..6) OPTIONAL,

 pusch-SPS-MaxConfigSubslot-r15 INTEGER (0..31) OPTIONAL,

 pusch-SPS-SlotRepPCell-r15 ENUMERATED {supported} OPTIONAL,

 pusch-SPS-SlotRepPSCell-r15 ENUMERATED {supported} OPTIONAL,

 pusch-SPS-SlotRepSCell-r15 ENUMERATED {supported} OPTIONAL,

 pusch-SPS-SubframeRepPCell-r15 ENUMERATED {supported} OPTIONAL,

 pusch-SPS-SubframeRepPSCell-r15 ENUMERATED {supported} OPTIONAL,

 pusch-SPS-SubframeRepSCell-r15 ENUMERATED {supported} OPTIONAL,

 pusch-SPS-SubslotRepPCell-r15 ENUMERATED {supported} OPTIONAL,

 pusch-SPS-SubslotRepPSCell-r15 ENUMERATED {supported} OPTIONAL,

 pusch-SPS-SubslotRepSCell-r15 ENUMERATED {supported} OPTIONAL,

 semiStaticCFI-r15 ENUMERATED {supported} OPTIONAL,

 semiStaticCFI-Pattern-r15 ENUMERATED {supported} OPTIONAL

 } OPTIONAL,

 altMCS-Table-r15 ENUMERATED {supported} OPTIONAL

}

PhyLayerParameters-v1540 ::= SEQUENCE {

 stti-SPT-Capabilities-v1540 SEQUENCE {

 slotPDSCH-TxDiv-TM8-r15 ENUMERATED {supported}

 } OPTIONAL,

 crs-IM-TM1-toTM9-OneRX-Port-v1540 ENUMERATED {supported} OPTIONAL,

 cch-IM-RefRecTypeA-OneRX-Port-v1540 ENUMERATED {supported} OPTIONAL

}

PhyLayerParameters-v1550 ::= SEQUENCE {

 dmrs-OverheadReduction-r15 ENUMERATED {supported} OPTIONAL

}

PhyLayerParameters-v1610 ::= SEQUENCE {

 ce-Capabilities-v1610 SEQUENCE {

 ce-CSI-RS-Feedback-r16 ENUMERATED {supported} OPTIONAL,

 ce-CSI-RS-FeedbackCodebookRestriction-r16 ENUMERATED {supported} OPTIONAL,

 crs-ChEstMPDCCH-CE-ModeA-r16 ENUMERATED {supported} OPTIONAL,

 crs-ChEstMPDCCH-CE-ModeB-r16 ENUMERATED {supported} OPTIONAL,

 crs-ChEstMPDCCH-CSI-r16 ENUMERATED {supported} OPTIONAL,

 crs-ChEstMPDCCH-ReciprocityTDD-r16 ENUMERATED {supported} OPTIONAL,

 etws-CMAS-RxInConnCE-ModeA-r16 ENUMERATED {supported} OPTIONAL,

 etws-CMAS-RxInConnCE-ModeB-r16 ENUMERATED {supported} OPTIONAL,

 mpdcch-InLteControlRegionCE-ModeA-r16 ENUMERATED {supported} OPTIONAL,

 mpdcch-InLteControlRegionCE-ModeB-r16 ENUMERATED {supported} OPTIONAL,

 pdsch-InLteControlRegionCE-ModeA-r16 ENUMERATED {supported} OPTIONAL,

 pdsch-InLteControlRegionCE-ModeB-r16 ENUMERATED {supported} OPTIONAL,

 multiTB-Parameters-r16 CE-MultiTB-Parameters-r16 OPTIONAL,

 resourceResvParameters-r16 CE-ResourceResvParameters-r16 OPTIONAL

 } OPTIONAL,

 widebandPRG-Slot-r16 ENUMERATED {supported} OPTIONAL,

 widebandPRG-Subslot-r16 ENUMERATED {supported} OPTIONAL,

 widebandPRG-Subframe-r16 ENUMERATED {supported} OPTIONAL,

 addSRS-r16 SEQUENCE {

 addSRS-FrequencyHopping-r16 ENUMERATED {supported} OPTIONAL,

 addSRS-AntennaSwitching-r16 ENUMERATED {useBasic} OPTIONAL,

 addSRS-CarrierSwitching-r16 ENUMERATED {supported} OPTIONAL

 } OPTIONAL,

 virtualCellID-BasicSRS-r16 ENUMERATED {supported} OPTIONAL,

 virtualCellID-AddSRS-r16 ENUMERATED {supported} OPTIONAL

}

PhyLayerParameters-v1700 ::= SEQUENCE {

 ce-Capabilities-v1700 SEQUENCE {

 ce-PDSCH-14HARQProcesses-r17 ENUMERATED {supported} OPTIONAL,

 ce-PDSCH-14HARQProcesses-Alt2-r17 ENUMERATED {supported} OPTIONAL,

 ce-PDSCH-MaxTBS-r17 ENUMERATED {supported} OPTIONAL

 } OPTIONAL

}

PhyLayerParameters-v1730 ::= SEQUENCE {

 csi-SubframeSet2ForDormantSCell-r17 ENUMERATED {supported} OPTIONAL

}

MIMO-UE-Parameters-r13 ::= SEQUENCE {

 parametersTM9-r13 MIMO-UE-ParametersPerTM-r13 OPTIONAL,

 parametersTM10-r13 MIMO-UE-ParametersPerTM-r13 OPTIONAL,

 srs-EnhancementsTDD-r13 ENUMERATED {supported} OPTIONAL,

 srs-Enhancements-r13 ENUMERATED {supported} OPTIONAL,

 interferenceMeasRestriction-r13 ENUMERATED {supported} OPTIONAL

}

MIMO-UE-Parameters-v13e0 ::= SEQUENCE {

 mimo-WeightedLayersCapabilities-r13 MIMO-WeightedLayersCapabilities-r13 OPTIONAL

}

MIMO-UE-Parameters-v1430 ::= SEQUENCE {

 parametersTM9-v1430 MIMO-UE-ParametersPerTM-v1430 OPTIONAL,

 parametersTM10-v1430 MIMO-UE-ParametersPerTM-v1430 OPTIONAL

}

MIMO-UE-Parameters-v1470 ::= SEQUENCE {

 parametersTM9-v1470 MIMO-UE-ParametersPerTM-v1470,

 parametersTM10-v1470 MIMO-UE-ParametersPerTM-v1470

}

MIMO-UE-ParametersPerTM-r13 ::= SEQUENCE {

 nonPrecoded-r13 MIMO-NonPrecodedCapabilities-r13 OPTIONAL,

 beamformed-r13 MIMO-UE-BeamformedCapabilities-r13 OPTIONAL,

 channelMeasRestriction-r13 ENUMERATED {supported} OPTIONAL,

 dmrs-Enhancements-r13 ENUMERATED {supported} OPTIONAL,

 csi-RS-EnhancementsTDD-r13 ENUMERATED {supported} OPTIONAL

}

MIMO-UE-ParametersPerTM-v1430 ::= SEQUENCE {

 nzp-CSI-RS-AperiodicInfo-r14 SEQUENCE {

 nMaxProc-r14 INTEGER(5..32),

 nMaxResource-r14 ENUMERATED {n1, n2, n4, n8}

 } OPTIONAL,

 nzp-CSI-RS-PeriodicInfo-r14 SEQUENCE {

 nMaxResource-r14 ENUMERATED {n1, n2, n4, n8}

 } OPTIONAL,

 zp-CSI-RS-AperiodicInfo-r14 ENUMERATED {supported} OPTIONAL,

 ul-dmrs-Enhancements-r14 ENUMERATED {supported} OPTIONAL,

 densityReductionNP-r14 ENUMERATED {supported} OPTIONAL,

 densityReductionBF-r14 ENUMERATED {supported} OPTIONAL,

 hybridCSI-r14 ENUMERATED {supported} OPTIONAL,

 semiOL-r14 ENUMERATED {supported} OPTIONAL,

 csi-ReportingNP-r14 ENUMERATED {supported} OPTIONAL,

 csi-ReportingAdvanced-r14 ENUMERATED {supported} OPTIONAL

}

MIMO-UE-ParametersPerTM-v1470 ::= SEQUENCE {

 csi-ReportingAdvancedMaxPorts-r14 ENUMERATED {n8, n12, n16, n20, n24, n28} OPTIONAL

}

MIMO-CA-ParametersPerBoBC-r13 ::= SEQUENCE {

 parametersTM9-r13 MIMO-CA-ParametersPerBoBCPerTM-r13 OPTIONAL,

 parametersTM10-r13 MIMO-CA-ParametersPerBoBCPerTM-r13 OPTIONAL

}

MIMO-CA-ParametersPerBoBC-r15 ::= SEQUENCE {

 parametersTM9-r15 MIMO-CA-ParametersPerBoBCPerTM-r15 OPTIONAL,

 parametersTM10-r15 MIMO-CA-ParametersPerBoBCPerTM-r15 OPTIONAL

}

MIMO-CA-ParametersPerBoBC-v1430 ::= SEQUENCE {

 parametersTM9-v1430 MIMO-CA-ParametersPerBoBCPerTM-v1430 OPTIONAL,

 parametersTM10-v1430 MIMO-CA-ParametersPerBoBCPerTM-v1430 OPTIONAL

}

MIMO-CA-ParametersPerBoBC-v1470 ::= SEQUENCE {

 parametersTM9-v1470 MIMO-CA-ParametersPerBoBCPerTM-v1470,

 parametersTM10-v1470 MIMO-CA-ParametersPerBoBCPerTM-v1470

}

MIMO-CA-ParametersPerBoBCPerTM-r13 ::= SEQUENCE {

 nonPrecoded-r13 MIMO-NonPrecodedCapabilities-r13 OPTIONAL,

 beamformed-r13 MIMO-BeamformedCapabilityList-r13 OPTIONAL,

 dmrs-Enhancements-r13 ENUMERATED {different} OPTIONAL

}

MIMO-CA-ParametersPerBoBCPerTM-v1430 ::= SEQUENCE {

 csi-ReportingNP-r14 ENUMERATED {different} OPTIONAL,

 csi-ReportingAdvanced-r14 ENUMERATED {different} OPTIONAL

}

MIMO-CA-ParametersPerBoBCPerTM-v1470 ::= SEQUENCE {

 csi-ReportingAdvancedMaxPorts-r14 ENUMERATED {n8, n12, n16, n20, n24, n28} OPTIONAL

}

MIMO-CA-ParametersPerBoBCPerTM-r15 ::= SEQUENCE {

 nonPrecoded-r13 MIMO-NonPrecodedCapabilities-r13 OPTIONAL,

 beamformed-r13 MIMO-BeamformedCapabilityList-r13 OPTIONAL,

 dmrs-Enhancements-r13 ENUMERATED {different} OPTIONAL,

 csi-ReportingNP-r14 ENUMERATED {different} OPTIONAL,

 csi-ReportingAdvanced-r14 ENUMERATED {different} OPTIONAL

}

MIMO-NonPrecodedCapabilities-r13 ::= SEQUENCE {

 config1-r13 ENUMERATED {supported} OPTIONAL,

 config2-r13 ENUMERATED {supported} OPTIONAL,

 config3-r13 ENUMERATED {supported} OPTIONAL,

 config4-r13 ENUMERATED {supported} OPTIONAL

}

MIMO-UE-BeamformedCapabilities-r13 ::= SEQUENCE {

 altCodebook-r13 ENUMERATED {supported} OPTIONAL,

 mimo-BeamformedCapabilities-r13 MIMO-BeamformedCapabilityList-r13

}

MIMO-BeamformedCapabilityList-r13 ::= SEQUENCE (SIZE (1..maxCSI-Proc-r11)) OF MIMO-BeamformedCapabilities-r13

MIMO-BeamformedCapabilities-r13 ::= SEQUENCE {

 k-Max-r13 INTEGER (1..8),

 n-MaxList-r13 BIT STRING (SIZE (1..7)) OPTIONAL

}

MIMO-WeightedLayersCapabilities-r13 ::= SEQUENCE {

 relWeightTwoLayers-r13 ENUMERATED {v1, v1dot25, v1dot5, v1dot75, v2, v2dot5, v3, v4},

 relWeightFourLayers-r13 ENUMERATED {v1, v1dot25, v1dot5, v1dot75, v2, v2dot5, v3, v4} OPTIONAL,

 relWeightEightLayers-r13 ENUMERATED {v1, v1dot25, v1dot5, v1dot75, v2, v2dot5, v3, v4} OPTIONAL,

 totalWeightedLayers-r13 INTEGER (2..128)

}

NonContiguousUL-RA-WithinCC-List-r10 ::= SEQUENCE (SIZE (1..maxBands)) OF NonContiguousUL-RA-WithinCC-r10

NonContiguousUL-RA-WithinCC-r10 ::= SEQUENCE {

 nonContiguousUL-RA-WithinCC-Info-r10 ENUMERATED {supported} OPTIONAL

}

RF-Parameters ::= SEQUENCE {

 supportedBandListEUTRA SupportedBandListEUTRA

}

RF-Parameters-v9e0 ::= SEQUENCE {

 supportedBandListEUTRA-v9e0 SupportedBandListEUTRA-v9e0 OPTIONAL

}

RF-Parameters-v1020 ::= SEQUENCE {

 supportedBandCombination-r10 SupportedBandCombination-r10

}

RF-Parameters-v1060 ::= SEQUENCE {

 supportedBandCombinationExt-r10 SupportedBandCombinationExt-r10

}

RF-Parameters-v1090 ::= SEQUENCE {

 supportedBandCombination-v1090 SupportedBandCombination-v1090 OPTIONAL

}

RF-Parameters-v10f0 ::= SEQUENCE {

 modifiedMPR-Behavior-r10 BIT STRING (SIZE (32)) OPTIONAL

}

RF-Parameters-v10i0 ::= SEQUENCE {

 supportedBandCombination-v10i0 SupportedBandCombination-v10i0 OPTIONAL

}

RF-Parameters-v10j0 ::= SEQUENCE {

 multiNS-Pmax-r10 ENUMERATED {supported} OPTIONAL

}

RF-Parameters-v1130 ::= SEQUENCE {

 supportedBandCombination-v1130 SupportedBandCombination-v1130 OPTIONAL

}

RF-Parameters-v1180 ::= SEQUENCE {

 freqBandRetrieval-r11 ENUMERATED {supported} OPTIONAL,

 requestedBands-r11 SEQUENCE (SIZE (1.. maxBands)) OF FreqBandIndicator-r11 OPTIONAL,

 supportedBandCombinationAdd-r11 SupportedBandCombinationAdd-r11 OPTIONAL

}

RF-Parameters-v11d0 ::= SEQUENCE {

 supportedBandCombinationAdd-v11d0 SupportedBandCombinationAdd-v11d0 OPTIONAL

}

RF-Parameters-v1250 ::= SEQUENCE {

 supportedBandListEUTRA-v1250 SupportedBandListEUTRA-v1250 OPTIONAL,

 supportedBandCombination-v1250 SupportedBandCombination-v1250 OPTIONAL,

 supportedBandCombinationAdd-v1250 SupportedBandCombinationAdd-v1250 OPTIONAL,

 freqBandPriorityAdjustment-r12 ENUMERATED {supported} OPTIONAL

}

RF-Parameters-v1270 ::= SEQUENCE {

 supportedBandCombination-v1270 SupportedBandCombination-v1270 OPTIONAL,

 supportedBandCombinationAdd-v1270 SupportedBandCombinationAdd-v1270 OPTIONAL

}

RF-Parameters-v1310 ::= SEQUENCE {

 eNB-RequestedParameters-r13 SEQUENCE {

 reducedIntNonContCombRequested-r13 ENUMERATED {true} OPTIONAL,

 requestedCCsDL-r13 INTEGER (2..32) OPTIONAL,

 requestedCCsUL-r13 INTEGER (2..32) OPTIONAL,

 skipFallbackCombRequested-r13 ENUMERATED {true} OPTIONAL

 } OPTIONAL,

 maximumCCsRetrieval-r13 ENUMERATED {supported} OPTIONAL,

 skipFallbackCombinations-r13 ENUMERATED {supported} OPTIONAL,

 reducedIntNonContComb-r13 ENUMERATED {supported} OPTIONAL,

 supportedBandListEUTRA-v1310 SupportedBandListEUTRA-v1310 OPTIONAL,

 supportedBandCombinationReduced-r13 SupportedBandCombinationReduced-r13 OPTIONAL

}

RF-Parameters-v1320 ::= SEQUENCE {

 supportedBandListEUTRA-v1320 SupportedBandListEUTRA-v1320 OPTIONAL,

 supportedBandCombination-v1320 SupportedBandCombination-v1320 OPTIONAL,

 supportedBandCombinationAdd-v1320 SupportedBandCombinationAdd-v1320 OPTIONAL,

 supportedBandCombinationReduced-v1320 SupportedBandCombinationReduced-v1320 OPTIONAL

}

RF-Parameters-v1380 ::= SEQUENCE {

 supportedBandCombination-v1380 SupportedBandCombination-v1380 OPTIONAL,

 supportedBandCombinationAdd-v1380 SupportedBandCombinationAdd-v1380 OPTIONAL,

 supportedBandCombinationReduced-v1380 SupportedBandCombinationReduced-v1380 OPTIONAL

}

RF-Parameters-v1390 ::= SEQUENCE {

 supportedBandCombination-v1390 SupportedBandCombination-v1390 OPTIONAL,

 supportedBandCombinationAdd-v1390 SupportedBandCombinationAdd-v1390 OPTIONAL,

 supportedBandCombinationReduced-v1390 SupportedBandCombinationReduced-v1390 OPTIONAL

}

RF-Parameters-v12b0 ::= SEQUENCE {

 maxLayersMIMO-Indication-r12 ENUMERATED {supported} OPTIONAL

}

RF-Parameters-v1430 ::= SEQUENCE {

 supportedBandCombination-v1430 SupportedBandCombination-v1430 OPTIONAL,

 supportedBandCombinationAdd-v1430 SupportedBandCombinationAdd-v1430 OPTIONAL,

 supportedBandCombinationReduced-v1430 SupportedBandCombinationReduced-v1430 OPTIONAL,

 eNB-RequestedParameters-v1430 SEQUENCE {

 requestedDiffFallbackCombList-r14 BandCombinationList-r14

 } OPTIONAL,

 diffFallbackCombReport-r14 ENUMERATED {supported} OPTIONAL

}

RF-Parameters-v1450 ::= SEQUENCE {

 supportedBandCombination-v1450 SupportedBandCombination-v1450 OPTIONAL,

 supportedBandCombinationAdd-v1450 SupportedBandCombinationAdd-v1450 OPTIONAL,

 supportedBandCombinationReduced-v1450 SupportedBandCombinationReduced-v1450 OPTIONAL

}

RF-Parameters-v1470 ::= SEQUENCE {

 supportedBandCombination-v1470 SupportedBandCombination-v1470 OPTIONAL,

 supportedBandCombinationAdd-v1470 SupportedBandCombinationAdd-v1470 OPTIONAL,

 supportedBandCombinationReduced-v1470 SupportedBandCombinationReduced-v1470 OPTIONAL

}

RF-Parameters-v14b0 ::= SEQUENCE {

 supportedBandCombination-v14b0 SupportedBandCombination-v14b0 OPTIONAL,

 supportedBandCombinationAdd-v14b0 SupportedBandCombinationAdd-v14b0 OPTIONAL,

 supportedBandCombinationReduced-v14b0 SupportedBandCombinationReduced-v14b0 OPTIONAL

}

RF-Parameters-v1530 ::= SEQUENCE {

 sTTI-SPT-Supported-r15 ENUMERATED {supported} OPTIONAL,

 supportedBandCombination-v1530 SupportedBandCombination-v1530 OPTIONAL,

 supportedBandCombinationAdd-v1530 SupportedBandCombinationAdd-v1530 OPTIONAL,

 supportedBandCombinationReduced-v1530 SupportedBandCombinationReduced-v1530 OPTIONAL,

 powerClass-14dBm-r15 ENUMERATED {supported} OPTIONAL

}

RF-Parameters-v1570 ::= SEQUENCE {

 dl-1024QAM-ScalingFactor-r15 ENUMERATED {v1, v1dot2, v1dot25},

 dl-1024QAM-TotalWeightedLayers-r15 INTEGER (0..10)

}

RF-Parameters-v1610 ::= SEQUENCE {

 supportedBandCombination-v1610 SupportedBandCombination-v1610 OPTIONAL,

 supportedBandCombinationAdd-v1610 SupportedBandCombinationAdd-v1610 OPTIONAL,

 supportedBandCombinationReduced-v1610 SupportedBandCombinationReduced-v1610 OPTIONAL

}

RF-Parameters-v1630 ::= SEQUENCE {

 supportedBandCombination-v1630 SupportedBandCombination-v1630 OPTIONAL,

 supportedBandCombinationAdd-v1630 SupportedBandCombinationAdd-v1630 OPTIONAL,

 supportedBandCombinationReduced-v1630 SupportedBandCombinationReduced-v1630 OPTIONAL

}

RF-Parameters-v1800 ::= SEQUENCE {

 -- Support handling of aerial-specific Ns and Pmax list broadcasted by the cell

 multiNS-PmaxAerial-r18 ENUMERATED {supported} OPTIONAL,

 supportedBandListEUTRA-v1800 SupportedBandListEUTRA-v1800 OPTIONAL,

 supportedBandCombination-v1800 SupportedBandCombination-v1800 OPTIONAL,

 supportedBandCombinationAdd-v1800 SupportedBandCombinationAdd-v1800 OPTIONAL,

 supportedBandCombinationReduced-v1800 SupportedBandCombinationReduced-v1800 OPTIONAL

}

SkipSubframeProcessing-r15 ::= SEQUENCE {

 skipProcessingDL-Slot-r15 INTEGER (0..3) OPTIONAL,

 skipProcessingDL-SubSlot-r15 INTEGER (0..3) OPTIONAL,

 skipProcessingUL-Slot-r15 INTEGER (0..3) OPTIONAL,

 skipProcessingUL-SubSlot-r15 INTEGER (0..3) OPTIONAL

}

SPT-Parameters-r15 ::= SEQUENCE {

 frameStructureType-SPT-r15 BIT STRING (SIZE (3)) OPTIONAL,

 maxNumberCCs-SPT-r15 INTEGER (1..32) OPTIONAL

}

STTI-SPT-BandParameters-r15 ::= SEQUENCE {

 dl-1024QAM-Slot-r15 ENUMERATED {supported} OPTIONAL,

 dl-1024QAM-SubslotTA-1-r15 ENUMERATED {supported} OPTIONAL,

 dl-1024QAM-SubslotTA-2-r15 ENUMERATED {supported} OPTIONAL,

 simultaneousTx-differentTx-duration-r15 ENUMERATED {supported} OPTIONAL,

 sTTI-CA-MIMO-ParametersDL-r15 CA-MIMO-ParametersDL-r15 OPTIONAL,

 sTTI-CA-MIMO-ParametersUL-r15 CA-MIMO-ParametersUL-r15,

 sTTI-FD-MIMO-Coexistence ENUMERATED {supported} OPTIONAL,

 sTTI-MIMO-CA-ParametersPerBoBCs-r15 MIMO-CA-ParametersPerBoBC-r13 OPTIONAL,

 sTTI-MIMO-CA-ParametersPerBoBCs-v1530 MIMO-CA-ParametersPerBoBC-v1430 OPTIONAL,

 sTTI-SupportedCombinations-r15 STTI-SupportedCombinations-r15 OPTIONAL,

 sTTI-SupportedCSI-Proc-r15 ENUMERATED {n1, n3, n4} OPTIONAL,

 ul-256QAM-Slot-r15 ENUMERATED {supported} OPTIONAL,

 ul-256QAM-Subslot-r15 ENUMERATED {supported} OPTIONAL,

 ...

}

STTI-SupportedCombinations-r15 ::= SEQUENCE {

 combination-22-r15 DL-UL-CCs-r15 OPTIONAL,

 combination-77-r15 DL-UL-CCs-r15 OPTIONAL,

 combination-27-r15 DL-UL-CCs-r15 OPTIONAL,

 combination-22-27-r15 SEQUENCE (SIZE (1..2)) OF DL-UL-CCs-r15 OPTIONAL,

 combination-77-22-r15 SEQUENCE (SIZE (1..2)) OF DL-UL-CCs-r15 OPTIONAL,

 combination-77-27-r15 SEQUENCE (SIZE (1..2)) OF DL-UL-CCs-r15 OPTIONAL

}

DL-UL-CCs-r15 ::= SEQUENCE {

 maxNumberDL-CCs-r15 INTEGER (1..32) OPTIONAL,

 maxNumberUL-CCs-r15 INTEGER (1..32) OPTIONAL

}

SupportedBandCombination-r10 ::= SEQUENCE (SIZE (1..maxBandComb-r10)) OF BandCombinationParameters-r10

SupportedBandCombinationExt-r10 ::= SEQUENCE (SIZE (1..maxBandComb-r10)) OF BandCombinationParametersExt-r10

SupportedBandCombination-v1090 ::= SEQUENCE (SIZE (1..maxBandComb-r10)) OF BandCombinationParameters-v1090

SupportedBandCombination-v10i0 ::= SEQUENCE (SIZE (1..maxBandComb-r10)) OF BandCombinationParameters-v10i0

SupportedBandCombination-v1130 ::= SEQUENCE (SIZE (1..maxBandComb-r10)) OF BandCombinationParameters-v1130

SupportedBandCombination-v1250 ::= SEQUENCE (SIZE (1..maxBandComb-r10)) OF BandCombinationParameters-v1250

SupportedBandCombination-v1270 ::= SEQUENCE (SIZE (1..maxBandComb-r10)) OF BandCombinationParameters-v1270

SupportedBandCombination-v1320 ::= SEQUENCE (SIZE (1..maxBandComb-r10)) OF BandCombinationParameters-v1320

SupportedBandCombination-v1380 ::= SEQUENCE (SIZE (1..maxBandComb-r10)) OF BandCombinationParameters-v1380

SupportedBandCombination-v1390 ::= SEQUENCE (SIZE (1..maxBandComb-r10)) OF BandCombinationParameters-v1390

SupportedBandCombination-v1430 ::= SEQUENCE (SIZE (1..maxBandComb-r10)) OF BandCombinationParameters-v1430

SupportedBandCombination-v1450 ::= SEQUENCE (SIZE (1..maxBandComb-r10)) OF BandCombinationParameters-v1450

SupportedBandCombination-v1470 ::= SEQUENCE (SIZE (1..maxBandComb-r10)) OF BandCombinationParameters-v1470

SupportedBandCombination-v14b0 ::= SEQUENCE (SIZE (1..maxBandComb-r10)) OF BandCombinationParameters-v14b0

SupportedBandCombination-v1530 ::= SEQUENCE (SIZE (1..maxBandComb-r10)) OF BandCombinationParameters-v1530

SupportedBandCombination-v1610 ::= SEQUENCE (SIZE (1..maxBandComb-r10)) OF BandCombinationParameters-v1610

SupportedBandCombination-v1630 ::= SEQUENCE (SIZE (1..maxBandComb-r10)) OF BandCombinationParameters-v1630

SupportedBandCombination-v1800 ::= SEQUENCE (SIZE (1..maxBandComb-r10)) OF BandCombinationParameters-v1800

SupportedBandCombinationAdd-r11 ::= SEQUENCE (SIZE (1..maxBandComb-r11)) OF BandCombinationParameters-r11

SupportedBandCombinationAdd-v11d0 ::= SEQUENCE (SIZE (1..maxBandComb-r11)) OF BandCombinationParameters-v10i0

SupportedBandCombinationAdd-v1250 ::= SEQUENCE (SIZE (1..maxBandComb-r11)) OF BandCombinationParameters-v1250

SupportedBandCombinationAdd-v1270 ::= SEQUENCE (SIZE (1..maxBandComb-r11)) OF BandCombinationParameters-v1270

SupportedBandCombinationAdd-v1320 ::= SEQUENCE (SIZE (1..maxBandComb-r11)) OF BandCombinationParameters-v1320

SupportedBandCombinationAdd-v1380 ::= SEQUENCE (SIZE (1..maxBandComb-r11)) OF BandCombinationParameters-v1380

SupportedBandCombinationAdd-v1390 ::= SEQUENCE (SIZE (1..maxBandComb-r11)) OF BandCombinationParameters-v1390

SupportedBandCombinationAdd-v1430 ::= SEQUENCE (SIZE (1..maxBandComb-r11)) OF BandCombinationParameters-v1430

SupportedBandCombinationAdd-v1450 ::= SEQUENCE (SIZE (1..maxBandComb-r11)) OF BandCombinationParameters-v1450

SupportedBandCombinationAdd-v1470 ::= SEQUENCE (SIZE (1..maxBandComb-r11)) OF BandCombinationParameters-v1470

SupportedBandCombinationAdd-v14b0 ::= SEQUENCE (SIZE (1..maxBandComb-r11)) OF BandCombinationParameters-v14b0

SupportedBandCombinationAdd-v1530 ::= SEQUENCE (SIZE (1..maxBandComb-r11)) OF BandCombinationParameters-v1530

SupportedBandCombinationAdd-v1610 ::= SEQUENCE (SIZE (1..maxBandComb-r11)) OF BandCombinationParameters-v1610

SupportedBandCombinationAdd-v1630 ::= SEQUENCE (SIZE (1..maxBandComb-r11)) OF BandCombinationParameters-v1630

SupportedBandCombinationAdd-v1800 ::= SEQUENCE (SIZE (1..maxBandComb-r11)) OF BandCombinationParameters-v1800

SupportedBandCombinationReduced-r13 ::= SEQUENCE (SIZE (1..maxBandComb-r13)) OF BandCombinationParameters-r13

SupportedBandCombinationReduced-v1320 ::= SEQUENCE (SIZE (1..maxBandComb-r13)) OF BandCombinationParameters-v1320

SupportedBandCombinationReduced-v1380 ::= SEQUENCE (SIZE (1..maxBandComb-r13)) OF BandCombinationParameters-v1380

SupportedBandCombinationReduced-v1390 ::= SEQUENCE (SIZE (1..maxBandComb-r13)) OF BandCombinationParameters-v1390

SupportedBandCombinationReduced-v1430 ::= SEQUENCE (SIZE (1..maxBandComb-r13)) OF BandCombinationParameters-v1430

SupportedBandCombinationReduced-v1450 ::= SEQUENCE (SIZE (1..maxBandComb-r13)) OF BandCombinationParameters-v1450

SupportedBandCombinationReduced-v1470 ::= SEQUENCE (SIZE (1..maxBandComb-r13)) OF BandCombinationParameters-v1470

SupportedBandCombinationReduced-v14b0 ::= SEQUENCE (SIZE (1..maxBandComb-r13)) OF BandCombinationParameters-v14b0

SupportedBandCombinationReduced-v1530 ::= SEQUENCE (SIZE (1..maxBandComb-r13)) OF BandCombinationParameters-v1530

SupportedBandCombinationReduced-v1610 ::= SEQUENCE (SIZE (1..maxBandComb-r13)) OF BandCombinationParameters-v1610

SupportedBandCombinationReduced-v1630 ::= SEQUENCE (SIZE (1..maxBandComb-r13)) OF BandCombinationParameters-v1630

SupportedBandCombinationReduced-v1800 ::= SEQUENCE (SIZE (1..maxBandComb-r13)) OF BandCombinationParameters-v1800

BandCombinationParameters-r10 ::= SEQUENCE (SIZE (1..maxSimultaneousBands-r10)) OF BandParameters-r10

BandCombinationParametersExt-r10 ::= SEQUENCE {

 supportedBandwidthCombinationSet-r10 SupportedBandwidthCombinationSet-r10 OPTIONAL

}

BandCombinationParameters-v1090 ::= SEQUENCE (SIZE (1..maxSimultaneousBands-r10)) OF BandParameters-v1090

BandCombinationParameters-v10i0::= SEQUENCE {

 bandParameterList-v10i0 SEQUENCE (SIZE (1..maxSimultaneousBands-r10)) OF

 BandParameters-v10i0 OPTIONAL

}

BandCombinationParameters-v1130 ::= SEQUENCE {

 multipleTimingAdvance-r11 ENUMERATED {supported} OPTIONAL,

 simultaneousRx-Tx-r11 ENUMERATED {supported} OPTIONAL,

 bandParameterList-r11 SEQUENCE (SIZE (1..maxSimultaneousBands-r10)) OF BandParameters-v1130 OPTIONAL,

 ...

}

BandCombinationParameters-r11 ::= SEQUENCE {

 bandParameterList-r11 SEQUENCE (SIZE (1..maxSimultaneousBands-r10)) OF

 BandParameters-r11,

 supportedBandwidthCombinationSet-r11 SupportedBandwidthCombinationSet-r10 OPTIONAL,

 multipleTimingAdvance-r11 ENUMERATED {supported} OPTIONAL,

 simultaneousRx-Tx-r11 ENUMERATED {supported} OPTIONAL,

 bandInfoEUTRA-r11 BandInfoEUTRA,

 ...

}

BandCombinationParameters-v1250::= SEQUENCE {

 dc-Support-r12 SEQUENCE {

 asynchronous-r12 ENUMERATED {supported} OPTIONAL,

 supportedCellGrouping-r12 CHOICE {

 threeEntries-r12 BIT STRING (SIZE(3)),

 fourEntries-r12 BIT STRING (SIZE(7)),

 fiveEntries-r12 BIT STRING (SIZE(15))

 } OPTIONAL

 } OPTIONAL,

 supportedNAICS-2CRS-AP-r12 BIT STRING (SIZE (1..maxNAICS-Entries-r12)) OPTIONAL,

 commSupportedBandsPerBC-r12 BIT STRING (SIZE (1.. maxBands)) OPTIONAL,

 ...

}

BandCombinationParameters-v1270 ::= SEQUENCE {

 bandParameterList-v1270 SEQUENCE (SIZE (1..maxSimultaneousBands-r10)) OF

 BandParameters-v1270 OPTIONAL

}

BandCombinationParameters-r13 ::= SEQUENCE {

 differentFallbackSupported-r13 ENUMERATED {true} OPTIONAL,

 bandParameterList-r13 SEQUENCE (SIZE (1..maxSimultaneousBands-r10)) OF BandParameters-r13,

 supportedBandwidthCombinationSet-r13 SupportedBandwidthCombinationSet-r10 OPTIONAL,

 multipleTimingAdvance-r13 ENUMERATED {supported} OPTIONAL,

 simultaneousRx-Tx-r13 ENUMERATED {supported} OPTIONAL,

 bandInfoEUTRA-r13 BandInfoEUTRA,

 dc-Support-r13 SEQUENCE {

 asynchronous-r13 ENUMERATED {supported} OPTIONAL,

 supportedCellGrouping-r13 CHOICE {

 threeEntries-r13 BIT STRING (SIZE(3)),

 fourEntries-r13 BIT STRING (SIZE(7)),

 fiveEntries-r13 BIT STRING (SIZE(15))

 } OPTIONAL

 } OPTIONAL,

 supportedNAICS-2CRS-AP-r13 BIT STRING (SIZE (1..maxNAICS-Entries-r12)) OPTIONAL,

 commSupportedBandsPerBC-r13 BIT STRING (SIZE (1.. maxBands)) OPTIONAL

}

BandCombinationParameters-v1320 ::= SEQUENCE {

 bandParameterList-v1320 SEQUENCE (SIZE (1..maxSimultaneousBands-r10)) OF

 BandParameters-v1320 OPTIONAL,

 additionalRx-Tx-PerformanceReq-r13 ENUMERATED {supported} OPTIONAL

}

BandCombinationParameters-v1380 ::= SEQUENCE {

 bandParameterList-v1380 SEQUENCE (SIZE (1..maxSimultaneousBands-r10)) OF

 BandParameters-v1380 OPTIONAL

}

BandCombinationParameters-v1390 ::= SEQUENCE {

 ue-CA-PowerClass-N-r13 ENUMERATED {class2} OPTIONAL

}

BandCombinationParameters-v1430 ::= SEQUENCE {

 bandParameterList-v1430 SEQUENCE (SIZE (1..maxSimultaneousBands-r10)) OF

 BandParameters-v1430 OPTIONAL,

 v2x-SupportedTxBandCombListPerBC-r14 BIT STRING (SIZE (1.. maxBandComb-r13)) OPTIONAL,

 v2x-SupportedRxBandCombListPerBC-r14 BIT STRING (SIZE (1.. maxBandComb-r13)) OPTIONAL

}

BandCombinationParameters-v1450 ::= SEQUENCE {

 bandParameterList-v1450 SEQUENCE (SIZE (1..maxSimultaneousBands-r10)) OF

 BandParameters-v1450 OPTIONAL

}

BandCombinationParameters-v1470 ::= SEQUENCE {

 bandParameterList-v1470 SEQUENCE (SIZE (1..maxSimultaneousBands-r10)) OF

 BandParameters-v1470 OPTIONAL,

 srs-MaxSimultaneousCCs-r14 INTEGER (1..31) OPTIONAL

}

BandCombinationParameters-v14b0 ::= SEQUENCE {

 bandParameterList-v14b0 SEQUENCE (SIZE (1..maxSimultaneousBands-r10)) OF

 BandParameters-v14b0 OPTIONAL

}

BandCombinationParameters-v1530 ::= SEQUENCE {

 bandParameterList-v1530 SEQUENCE (SIZE (1..maxSimultaneousBands-r10)) OF BandParameters-v1530 OPTIONAL,

 spt-Parameters-r15 SPT-Parameters-r15 OPTIONAL

}

-- If an additional band combination parameter is defined, which is supported for MR-DC,

-- it shall be defined in the IE CA-ParametersEUTRA in TS 38.331 [82].

BandCombinationParameters-v1610 ::= SEQUENCE {

 measGapInfoNR-r16 MeasGapInfoNR-r16 OPTIONAL,

 bandParameterList-v1610 SEQUENCE (SIZE (1..maxSimultaneousBands-r10)) OF BandParameters-v1610 OPTIONAL,

 interFreqDAPS-r16 SEQUENCE {

 interFreqAsyncDAPS-r16 ENUMERATED {supported} OPTIONAL,

 interFreqMultiUL-TransmissionDAPS-r16 ENUMERATED {supported} OPTIONAL

 } OPTIONAL

}

BandCombinationParameters-v1630 ::= SEQUENCE {

 v2x-SupportedTxBandCombListPerBC-v1630 BIT STRING (SIZE (1..maxBandCombSidelinkNR-r16)) OPTIONAL,

 v2x-SupportedRxBandCombListPerBC-v1630 BIT STRING (SIZE (1..maxBandCombSidelinkNR-r16)) OPTIONAL,

 scalingFactorTxSidelink-r16 SEQUENCE (SIZE (1..maxBandCombSidelinkNR-r16)) OF ScalingFactorSidelink-r16 OPTIONAL,

 scalingFactorRxSidelink-r16 SEQUENCE (SIZE (1..maxBandCombSidelinkNR-r16)) OF ScalingFactorSidelink-r16 OPTIONAL,

 interBandPowerSharingSyncDAPS-r16 ENUMERATED {supported} OPTIONAL,

 interBandPowerSharingAsyncDAPS-r16 ENUMERATED {supported} OPTIONAL

}

BandCombinationParameters-v1800 ::= SEQUENCE {

 measGapInfoNR-r18 MeasGapInfoNR-r18 OPTIONAL

}

ScalingFactorSidelink-r16 ::= ENUMERATED {f0p4, f0p75, f0p8, f1}

SupportedBandwidthCombinationSet-r10 ::= BIT STRING (SIZE (1..maxBandwidthCombSet-r10))

BandParameters-r10 ::= SEQUENCE {

 bandEUTRA-r10 FreqBandIndicator,

 bandParametersUL-r10 BandParametersUL-r10 OPTIONAL,

 bandParametersDL-r10 BandParametersDL-r10 OPTIONAL

}

BandParameters-v1090 ::= SEQUENCE {

 bandEUTRA-v1090 FreqBandIndicator-v9e0 OPTIONAL,

 ...

}

BandParameters-v10i0::= SEQUENCE {

 bandParametersDL-v10i0 SEQUENCE (SIZE (1..maxBandwidthClass-r10)) OF CA-MIMO-ParametersDL-v10i0

}

BandParameters-v1130 ::= SEQUENCE {

 supportedCSI-Proc-r11 ENUMERATED {n1, n3, n4}

}

BandParameters-r11 ::= SEQUENCE {

 bandEUTRA-r11 FreqBandIndicator-r11,

 bandParametersUL-r11 BandParametersUL-r10 OPTIONAL,

 bandParametersDL-r11 BandParametersDL-r10 OPTIONAL,

 supportedCSI-Proc-r11 ENUMERATED {n1, n3, n4} OPTIONAL

}

BandParameters-v1270 ::= SEQUENCE {

 bandParametersDL-v1270 SEQUENCE (SIZE (1..maxBandwidthClass-r10)) OF CA-MIMO-ParametersDL-v1270

}

BandParameters-r13 ::= SEQUENCE {

 bandEUTRA-r13 FreqBandIndicator-r11,

 bandParametersUL-r13 BandParametersUL-r13 OPTIONAL,

 bandParametersDL-r13 BandParametersDL-r13 OPTIONAL,

 supportedCSI-Proc-r13 ENUMERATED {n1, n3, n4} OPTIONAL

}

BandParameters-v1320 ::= SEQUENCE {

 bandParametersDL-v1320 MIMO-CA-ParametersPerBoBC-r13

}

BandParameters-v1380 ::= SEQUENCE {

 txAntennaSwitchDL-r13 INTEGER (1..32) OPTIONAL,

 txAntennaSwitchUL-r13 INTEGER (1..32) OPTIONAL

}

BandParameters-v1430 ::= SEQUENCE {

 bandParametersDL-v1430 MIMO-CA-ParametersPerBoBC-v1430 OPTIONAL,

 ul-256QAM-r14 ENUMERATED {supported} OPTIONAL,

 ul-256QAM-perCC-InfoList-r14 SEQUENCE (SIZE (2..maxServCell-r13)) OF UL-256QAM-perCC-Info-r14 OPTIONAL,

 srs-CapabilityPerBandPairList-r14 SEQUENCE (SIZE (1..maxSimultaneousBands-r10)) OF

 SRS-CapabilityPerBandPair-r14 OPTIONAL

}

BandParameters-v1450 ::= SEQUENCE {

 must-CapabilityPerBand-r14 MUST-Parameters-r14 OPTIONAL

}

BandParameters-v1470 ::= SEQUENCE {

 bandParametersDL-v1470 MIMO-CA-ParametersPerBoBC-v1470 OPTIONAL

}

BandParameters-v14b0 ::= SEQUENCE {

 srs-CapabilityPerBandPairList-v14b0 SEQUENCE (SIZE (1..maxSimultaneousBands-r10)) OF SRS-CapabilityPerBandPair-v14b0 OPTIONAL

}

BandParameters-v1530 ::= SEQUENCE {

 ue-TxAntennaSelection-SRS-1T4R-r15 ENUMERATED {supported} OPTIONAL,

 ue-TxAntennaSelection-SRS-2T4R-2Pairs-r15 ENUMERATED {supported} OPTIONAL,

 ue-TxAntennaSelection-SRS-2T4R-3Pairs-r15 ENUMERATED {supported} OPTIONAL,

 dl-1024QAM-r15 ENUMERATED {supported} OPTIONAL,

 qcl-TypeC-Operation-r15 ENUMERATED {supported} OPTIONAL,

 qcl-CRI-BasedCSI-Reporting-r15 ENUMERATED {supported} OPTIONAL,

 stti-SPT-BandParameters-r15 STTI-SPT-BandParameters-r15 OPTIONAL

}

BandParameters-v1610 ::= SEQUENCE {

 intraFreqDAPS-r16 SEQUENCE {

 intraFreqAsyncDAPS-r16 ENUMERATED {supported} OPTIONAL,

 dummy ENUMERATED {supported} OPTIONAL,

 intraFreqTwoTAGs-DAPS-r16 ENUMERATED {supported} OPTIONAL

 } OPTIONAL,

 addSRS-FrequencyHopping-r16 ENUMERATED {supported} OPTIONAL,

 addSRS-AntennaSwitching-r16 SEQUENCE {

 addSRS-1T2R-r16 ENUMERATED {supported} OPTIONAL,

 addSRS-1T4R-r16 ENUMERATED {supported} OPTIONAL,

 addSRS-2T4R-2pairs-r16 ENUMERATED {supported} OPTIONAL,

 addSRS-2T4R-3pairs-r16 ENUMERATED {supported} OPTIONAL

 } OPTIONAL,

 srs-CapabilityPerBandPairList-v1610 SEQUENCE (SIZE (1..maxSimultaneousBands-r10)) OF

 SRS-CapabilityPerBandPair-v1610 OPTIONAL

}

V2X-BandParameters-r14 ::= SEQUENCE {

 v2x-FreqBandEUTRA-r14 FreqBandIndicator-r11,

 bandParametersTxSL-r14 BandParametersTxSL-r14 OPTIONAL,

 bandParametersRxSL-r14 BandParametersRxSL-r14 OPTIONAL

}

V2X-BandParameters-v1530 ::= SEQUENCE {

 v2x-EnhancedHighReception-r15 ENUMERATED {supported} OPTIONAL

}

BandParametersTxSL-r14 ::= SEQUENCE {

 v2x-BandwidthClassTxSL-r14 V2X-BandwidthClassSL-r14,

 v2x-eNB-Scheduled-r14 ENUMERATED {supported} OPTIONAL,

 v2x-HighPower-r14 ENUMERATED {supported} OPTIONAL

}

BandParametersRxSL-r14 ::= SEQUENCE {

 v2x-BandwidthClassRxSL-r14 V2X-BandwidthClassSL-r14,

 v2x-HighReception-r14 ENUMERATED {supported} OPTIONAL

}

V2X-BandwidthClassSL-r14 ::= SEQUENCE (SIZE (1..maxBandwidthClass-r10)) OF V2X-BandwidthClass-r14

UL-256QAM-perCC-Info-r14 ::= SEQUENCE {

 ul-256QAM-perCC-r14 ENUMERATED {supported} OPTIONAL

}

FeatureSetDL-r15 ::= SEQUENCE {

 mimo-CA-ParametersPerBoBC-r15 MIMO-CA-ParametersPerBoBC-r15 OPTIONAL,

 featureSetPerCC-ListDL-r15 SEQUENCE (SIZE (1..maxServCell-r13)) OF FeatureSetDL-PerCC-Id-r15

}

FeatureSetDL-v1550 ::= SEQUENCE {

 dl-1024QAM-r15 ENUMERATED {supported} OPTIONAL

}

FeatureSetDL-PerCC-r15 ::= SEQUENCE {

 fourLayerTM3-TM4-r15 ENUMERATED {supported} OPTIONAL,

 supportedMIMO-CapabilityDL-MRDC-r15 MIMO-CapabilityDL-r10 OPTIONAL,

 supportedCSI-Proc-r15 ENUMERATED {n1, n3, n4} OPTIONAL

}

FeatureSetUL-r15 ::= SEQUENCE {

 featureSetPerCC-ListUL-r15 SEQUENCE (SIZE(1..maxServCell-r13)) OF FeatureSetUL-PerCC-Id-r15

}

FeatureSetUL-PerCC-r15 ::= SEQUENCE {

 supportedMIMO-CapabilityUL-r15 MIMO-CapabilityUL-r10 OPTIONAL,

 ul-256QAM-r15 ENUMERATED {supported} OPTIONAL

}

FeatureSetDL-PerCC-Id-r15 ::= INTEGER (0..maxPerCC-FeatureSets-r15)

FeatureSetUL-PerCC-Id-r15 ::= INTEGER (0..maxPerCC-FeatureSets-r15)

BandParametersUL-r10 ::= SEQUENCE (SIZE (1..maxBandwidthClass-r10)) OF CA-MIMO-ParametersUL-r10

BandParametersUL-r13 ::= CA-MIMO-ParametersUL-r10

CA-MIMO-ParametersUL-r10 ::= SEQUENCE {

 ca-BandwidthClassUL-r10 CA-BandwidthClass-r10,

 supportedMIMO-CapabilityUL-r10 MIMO-CapabilityUL-r10 OPTIONAL

}

CA-MIMO-ParametersUL-r15 ::= SEQUENCE {

 supportedMIMO-CapabilityUL-r15 MIMO-CapabilityUL-r10 OPTIONAL

}

BandParametersDL-r10 ::= SEQUENCE (SIZE (1..maxBandwidthClass-r10)) OF CA-MIMO-ParametersDL-r10

BandParametersDL-r13 ::= CA-MIMO-ParametersDL-r13

CA-MIMO-ParametersDL-r10 ::= SEQUENCE {

 ca-BandwidthClassDL-r10 CA-BandwidthClass-r10,

 supportedMIMO-CapabilityDL-r10 MIMO-CapabilityDL-r10 OPTIONAL

}

CA-MIMO-ParametersDL-v10i0 ::= SEQUENCE {

 fourLayerTM3-TM4-r10 ENUMERATED {supported} OPTIONAL

}

CA-MIMO-ParametersDL-v1270 ::= SEQUENCE {

 intraBandContiguousCC-InfoList-r12 SEQUENCE (SIZE (1..maxServCell-r10)) OF IntraBandContiguousCC-Info-r12

}

CA-MIMO-ParametersDL-r13 ::= SEQUENCE {

 ca-BandwidthClassDL-r13 CA-BandwidthClass-r10,

 supportedMIMO-CapabilityDL-r13 MIMO-CapabilityDL-r10 OPTIONAL,

 fourLayerTM3-TM4-r13 ENUMERATED {supported} OPTIONAL,

 intraBandContiguousCC-InfoList-r13 SEQUENCE (SIZE (1..maxServCell-r13)) OF IntraBandContiguousCC-Info-r12

}

CA-MIMO-ParametersDL-r15 ::= SEQUENCE {

 supportedMIMO-CapabilityDL-r15 MIMO-CapabilityDL-r10 OPTIONAL,

 fourLayerTM3-TM4-r15 ENUMERATED {supported} OPTIONAL,

 intraBandContiguousCC-InfoList-r15 SEQUENCE (SIZE (1..maxServCell-r13)) OF

 IntraBandContiguousCC-Info-r12 OPTIONAL

}

IntraBandContiguousCC-Info-r12 ::= SEQUENCE {

 fourLayerTM3-TM4-perCC-r12 ENUMERATED {supported} OPTIONAL,

 supportedMIMO-CapabilityDL-r12 MIMO-CapabilityDL-r10 OPTIONAL,

 supportedCSI-Proc-r12 ENUMERATED {n1, n3, n4} OPTIONAL

}

CA-BandwidthClass-r10 ::= ENUMERATED {a, b, c, d, e, f, ...}

V2X-BandwidthClass-r14 ::= ENUMERATED {a, b, c, d, e, f, ..., c1-v1530}

MIMO-CapabilityUL-r10 ::= ENUMERATED {twoLayers, fourLayers}

MIMO-CapabilityDL-r10 ::= ENUMERATED {twoLayers, fourLayers, eightLayers}

MUST-Parameters-r14 ::= SEQUENCE {

 must-TM234-UpTo2Tx-r14 ENUMERATED {supported} OPTIONAL,

 must-TM89-UpToOneInterferingLayer-r14 ENUMERATED {supported} OPTIONAL,

 must-TM10-UpToOneInterferingLayer-r14 ENUMERATED {supported} OPTIONAL,

 must-TM89-UpToThreeInterferingLayers-r14 ENUMERATED {supported} OPTIONAL,

 must-TM10-UpToThreeInterferingLayers-r14 ENUMERATED {supported} OPTIONAL

}

SupportedBandListEUTRA ::= SEQUENCE (SIZE (1..maxBands)) OF SupportedBandEUTRA

SupportedBandListEUTRA-v9e0::= SEQUENCE (SIZE (1..maxBands)) OF SupportedBandEUTRA-v9e0

SupportedBandListEUTRA-v1250 ::= SEQUENCE (SIZE (1..maxBands)) OF SupportedBandEUTRA-v1250

SupportedBandListEUTRA-v1310 ::= SEQUENCE (SIZE (1..maxBands)) OF SupportedBandEUTRA-v1310

SupportedBandListEUTRA-v1320 ::= SEQUENCE (SIZE (1..maxBands)) OF SupportedBandEUTRA-v1320

SupportedBandListEUTRA-v1800 ::= SEQUENCE (SIZE (1..maxBands)) OF SupportedBandEUTRA-v1800

SupportedBandEUTRA ::= SEQUENCE {

 bandEUTRA FreqBandIndicator,

 halfDuplex BOOLEAN

}

SupportedBandEUTRA-v9e0 ::= SEQUENCE {

 bandEUTRA-v9e0 FreqBandIndicator-v9e0 OPTIONAL

}

SupportedBandEUTRA-v1250 ::= SEQUENCE {

 dl-256QAM-r12 ENUMERATED {supported} OPTIONAL,

 ul-64QAM-r12 ENUMERATED {supported} OPTIONAL

}

SupportedBandEUTRA-v1310 ::= SEQUENCE {

 ue-PowerClass-5-r13 ENUMERATED {supported} OPTIONAL

}

SupportedBandEUTRA-v1320 ::= SEQUENCE {

 intraFreq-CE-NeedForGaps-r13 ENUMERATED {supported} OPTIONAL,

 ue-PowerClass-N-r13 ENUMERATED {class1, class2, class4} OPTIONAL

}

SupportedBandEUTRA-v1800 ::= SEQUENCE {

 lowerMSD-MRDC-r18 SEQUENCE (SIZE (1..maxLowerMSD-r18)) OF LowerMSD-MRDC-r18 OPTIONAL

}

MeasParameters ::= SEQUENCE {

 bandListEUTRA BandListEUTRA

}

MeasParameters-v1020 ::= SEQUENCE {

 bandCombinationListEUTRA-r10 BandCombinationListEUTRA-r10

}

MeasParameters-v1130 ::= SEQUENCE {

 rsrqMeasWideband-r11 ENUMERATED {supported} OPTIONAL

}

MeasParameters-v11a0 ::= SEQUENCE {

 benefitsFromInterruption-r11 ENUMERATED {true} OPTIONAL

}

MeasParameters-v1250 ::= SEQUENCE {

 timerT312-r12 ENUMERATED {supported} OPTIONAL,

 alternativeTimeToTrigger-r12 ENUMERATED {supported} OPTIONAL,

 incMonEUTRA-r12 ENUMERATED {supported} OPTIONAL,

 incMonUTRA-r12 ENUMERATED {supported} OPTIONAL,

 extendedMaxMeasId-r12 ENUMERATED {supported} OPTIONAL,

 extendedRSRQ-LowerRange-r12 ENUMERATED {supported} OPTIONAL,

 rsrq-OnAllSymbols-r12 ENUMERATED {supported} OPTIONAL,

 crs-DiscoverySignalsMeas-r12 ENUMERATED {supported} OPTIONAL,

 csi-RS-DiscoverySignalsMeas-r12 ENUMERATED {supported} OPTIONAL

}

MeasParameters-v1310 ::= SEQUENCE {

 rs-SINR-Meas-r13 ENUMERATED {supported} OPTIONAL,

 allowedCellList-r13 ENUMERATED {supported} OPTIONAL,

 extendedMaxObjectId-r13 ENUMERATED {supported} OPTIONAL,

 ul-PDCP-Delay-r13 ENUMERATED {supported} OPTIONAL,

 extendedFreqPriorities-r13 ENUMERATED {supported} OPTIONAL,

 multiBandInfoReport-r13 ENUMERATED {supported} OPTIONAL,

 rssi-AndChannelOccupancyReporting-r13 ENUMERATED {supported} OPTIONAL

}

MeasParameters-v1430 ::= SEQUENCE {

 ceMeasurements-r14 ENUMERATED {supported} OPTIONAL,

 ncsg-r14 ENUMERATED {supported} OPTIONAL,

 shortMeasurementGap-r14 ENUMERATED {supported} OPTIONAL,

 perServingCellMeasurementGap-r14 ENUMERATED {supported} OPTIONAL,

 nonUniformGap-r14 ENUMERATED {supported} OPTIONAL

}

MeasParameters-v1520 ::= SEQUENCE {

 measGapPatterns-r15 BIT STRING (SIZE (8)) OPTIONAL

}

MeasParameters-v1530 ::= SEQUENCE {

 qoe-MeasReport-r15 ENUMERATED {supported} OPTIONAL,

 qoe-MTSI-MeasReport-r15 ENUMERATED {supported} OPTIONAL,

 ca-IdleModeMeasurements-r15 ENUMERATED {supported} OPTIONAL,

 ca-IdleModeValidityArea-r15 ENUMERATED {supported} OPTIONAL,

 heightMeas-r15 ENUMERATED {supported} OPTIONAL,

 multipleCellsMeasExtension-r15 ENUMERATED {supported} OPTIONAL

}

MeasParameters-v1610 ::= SEQUENCE {

 bandInfoNR-v1610 SEQUENCE (SIZE (1..maxBands)) OF MeasGapInfoNR-r16 OPTIONAL,

 altFreqPriority-r16 ENUMERATED {supported} OPTIONAL,

 ce-DL-ChannelQualityReporting-r16 ENUMERATED {supported} OPTIONAL,

 ce-MeasRSS-Dedicated-r16 ENUMERATED {supported} OPTIONAL,

 eutra-IdleInactiveMeasurements-r16 ENUMERATED {supported} OPTIONAL,

 nr-IdleInactiveMeasFR1-r16 ENUMERATED {supported} OPTIONAL,

 nr-IdleInactiveMeasFR2-r16 ENUMERATED {supported} OPTIONAL,

 idleInactiveValidityAreaList-r16 ENUMERATED {supported} OPTIONAL,

 measGapPatterns-NRonly-r16 ENUMERATED {supported} OPTIONAL,

 measGapPatterns-NRonly-ENDC-r16 ENUMERATED {supported} OPTIONAL

}

MeasParameters-v1630 ::= SEQUENCE {

 nr-IdleInactiveBeamMeasFR1-r16 ENUMERATED {supported} OPTIONAL,

 nr-IdleInactiveBeamMeasFR2-r16 ENUMERATED {supported} OPTIONAL,

 ce-MeasRSS-DedicatedSameRBs-r16 ENUMERATED {supported} OPTIONAL

}

MeasParameters-v16c0 ::= SEQUENCE {

 nr-CellIndividualOffset-r16 ENUMERATED {supported} OPTIONAL

}

MeasParameters-v1700 ::= SEQUENCE {

 sharedSpectrumMeasNR-EN-DC-r17 SEQUENCE (SIZE (1..maxBandsNR-r15)) OF SharedSpectrumMeasNR-r17 OPTIONAL,

 sharedSpectrumMeasNR-SA-r17 SEQUENCE (SIZE (1..maxBandsNR-r15)) OF SharedSpectrumMeasNR-r17 OPTIONAL

}

MeasParameters-v1770 ::= SEQUENCE {

 gaplessMeas-FR2-maxCC-r17 INTEGER (1..32) OPTIONAL

}

MeasParameters-v1800 ::= SEQUENCE {

 bandInfoNR-v1800 SEQUENCE (SIZE (1..maxBands)) OF MeasGapInfoNR-r18

}

MeasParameters-v1840 ::= SEQUENCE {

 simultaneousRxDataSSB-DiffNumerology-FR1-r18 ENUMERATED {supported} OPTIONAL

}

SharedSpectrumMeasNR-r17 ::= SEQUENCE {

 nr-RSSI-ChannelOccupancyReporting-r17 BOOLEAN

}

MeasGapInfoNR-r16 ::= SEQUENCE {

 interRAT-BandListNR-EN-DC-r16 InterRAT-BandListNR-r16 OPTIONAL,

 interRAT-BandListNR-SA-r16 InterRAT-BandListNR-r16 OPTIONAL

}

MeasGapInfoNR-r18 ::= SEQUENCE {

 interRAT-BandListNR-EN-DC-r18 InterRAT-BandListNR-r18 OPTIONAL,

 interRAT-BandListNR-SA-r18 InterRAT-BandListNR-r18 OPTIONAL

}

BandListEUTRA ::= SEQUENCE (SIZE (1..maxBands)) OF BandInfoEUTRA

BandCombinationListEUTRA-r10 ::= SEQUENCE (SIZE (1..maxBandComb-r10)) OF BandInfoEUTRA

BandInfoEUTRA ::= SEQUENCE {

 interFreqBandList InterFreqBandList,

 interRAT-BandList InterRAT-BandList OPTIONAL

}

InterFreqBandList ::= SEQUENCE (SIZE (1..maxBands)) OF InterFreqBandInfo

InterFreqBandInfo ::= SEQUENCE {

 interFreqNeedForGaps BOOLEAN

}

InterRAT-BandList ::= SEQUENCE (SIZE (1..maxBands)) OF InterRAT-BandInfo

InterRAT-BandListNR-r16 ::= SEQUENCE (SIZE (1..maxBandsNR-r15)) OF InterRAT-BandInfoNR-r16

InterRAT-BandListNR-r18 ::= SEQUENCE (SIZE (1..maxBandsNR-r15)) OF InterRAT-BandInfoNR-r18

InterRAT-BandInfo ::= SEQUENCE {

 interRAT-NeedForGaps BOOLEAN

}

InterRAT-BandInfoNR-r16 ::= SEQUENCE {

 interRAT-NeedForGapsNR-r16 BOOLEAN

}

InterRAT-BandInfoNR-r18 ::= SEQUENCE {

 interRAT-NeedForInterruptionNR-r18

 ENUMERATED {no-gap-with-interruption, no-gap-no-interruption} OPTIONAL

}

IRAT-ParametersNR-r15 ::= SEQUENCE {

 en-DC-r15 ENUMERATED {supported} OPTIONAL,

 eventB2-r15 ENUMERATED {supported} OPTIONAL,

 supportedBandListEN-DC-r15 SupportedBandListNR-r15 OPTIONAL

}

IRAT-ParametersNR-v1540 ::= SEQUENCE {

 eutra-5GC-HO-ToNR-FDD-FR1-r15 ENUMERATED {supported} OPTIONAL,

 eutra-5GC-HO-ToNR-TDD-FR1-r15 ENUMERATED {supported} OPTIONAL,

 eutra-5GC-HO-ToNR-FDD-FR2-r15 ENUMERATED {supported} OPTIONAL,

 eutra-5GC-HO-ToNR-TDD-FR2-r15 ENUMERATED {supported} OPTIONAL,

 eutra-EPC-HO-ToNR-FDD-FR1-r15 ENUMERATED {supported} OPTIONAL,

 eutra-EPC-HO-ToNR-TDD-FR1-r15 ENUMERATED {supported} OPTIONAL,

 eutra-EPC-HO-ToNR-FDD-FR2-r15 ENUMERATED {supported} OPTIONAL,

 eutra-EPC-HO-ToNR-TDD-FR2-r15 ENUMERATED {supported} OPTIONAL,

 ims-VoiceOverNR-FR1-r15 ENUMERATED {supported} OPTIONAL,

 ims-VoiceOverNR-FR2-r15 ENUMERATED {supported} OPTIONAL,

 sa-NR-r15 ENUMERATED {supported} OPTIONAL,

 supportedBandListNR-SA-r15 SupportedBandListNR-r15 OPTIONAL

}

IRAT-ParametersNR-v1560 ::= SEQUENCE {

 ng-EN-DC-r15 ENUMERATED {supported} OPTIONAL

}

IRAT-ParametersNR-v1570 ::= SEQUENCE {

 ss-SINR-Meas-NR-FR1-r15 ENUMERATED {supported} OPTIONAL,

 ss-SINR-Meas-NR-FR2-r15 ENUMERATED {supported} OPTIONAL

}

IRAT-ParametersNR-v1610 ::= SEQUENCE {

 nr-HO-ToEN-DC-r16 ENUMERATED {supported} OPTIONAL,

 ce-EUTRA-5GC-HO-ToNR-FDD-FR1-r16 ENUMERATED {supported} OPTIONAL,

 ce-EUTRA-5GC-HO-ToNR-TDD-FR1-r16 ENUMERATED {supported} OPTIONAL,

 ce-EUTRA-5GC-HO-ToNR-FDD-FR2-r16 ENUMERATED {supported} OPTIONAL,

 ce-EUTRA-5GC-HO-ToNR-TDD-FR2-r16 ENUMERATED {supported} OPTIONAL

}

IRAT-ParametersNR-v1660 ::= SEQUENCE {

 extendedBand-n77-r16 ENUMERATED {supported} OPTIONAL

}

IRAT-ParametersNR-v1700 ::= SEQUENCE {

 eutra-5GC-HO-ToNR-TDD-FR2-2-r17 ENUMERATED {supported} OPTIONAL,

 eutra-EPC-HO-ToNR-TDD-FR2-2-r17 ENUMERATED {supported} OPTIONAL,

 ce-EUTRA-5GC-HO-ToNR-TDD-FR2-2-r17 ENUMERATED {supported} OPTIONAL,

 ims-VoiceOverNR-FR2-2-r17 ENUMERATED {supported} OPTIONAL

}

IRAT-ParametersNR-v1710 ::= SEQUENCE {

 extendedBand-n77-2-r17 ENUMERATED {supported} OPTIONAL

}

IRAT-ParametersNR-v19xy ::= SEQUENCE {

 ntn-MeasForNR-r19 ENUMERATED {supported} OPTIONAL

}

LowerMSD-MRDC-r18 ::= SEQUENCE {

 aggressorband1-r18 FreqBandIndicatorNR-r15,

 aggressorband2-r18 FreqBandIndicator-r11 OPTIONAL,

 msd-Information-r18 SEQUENCE (SIZE (1.. maxLowerMSD-Info-r18)) OF MSD-Information-r18

}

MSD-Information-r18 ::= SEQUENCE {

 msd-Type-r18 ENUMERATED {harmonic, harmonicMixing, crossBandIsolation, imd2,

 imd3, imd4, imd5, all, spare8, spare7, spare6,

 spare5,spare4, spare3, spare2, spare1},

 msd-PowerClass-r18 ENUMERATED {pc1dot5, pc2, pc3},

 msd-Class-r18 ENUMERATED {classI, classII, classIII, classIV, classV, classVI,

 classVII, classVIII }

}

EUTRA-5GC-Parameters-r15 ::= SEQUENCE {

 eutra-5GC-r15 ENUMERATED {supported} OPTIONAL,

 eutra-EPC-HO-EUTRA-5GC-r15 ENUMERATED {supported} OPTIONAL,

 ho-EUTRA-5GC-FDD-TDD-r15 ENUMERATED {supported} OPTIONAL,

 ho-InterfreqEUTRA-5GC-r15 ENUMERATED {supported} OPTIONAL,

 ims-VoiceOverMCG-BearerEUTRA-5GC-r15 ENUMERATED {supported} OPTIONAL,

 inactiveState-r15 ENUMERATED {supported} OPTIONAL,

 reflectiveQoS-r15 ENUMERATED {supported} OPTIONAL

}

EUTRA-5GC-Parameters-v1610 ::= SEQUENCE {

 ce-InactiveState-r16 ENUMERATED {supported} OPTIONAL,

 ce-EUTRA-5GC-r16 ENUMERATED {supported} OPTIONAL

}

PDCP-ParametersNR-r15 ::= SEQUENCE {

 rohc-Profiles-r15 ROHC-ProfileSupportList-r15,

 rohc-ContextMaxSessions-r15 ENUMERATED {

 cs2, cs4, cs8, cs12, cs16, cs24, cs32,

 cs48, cs64, cs128, cs256, cs512, cs1024,

 cs16384, spare2, spare1} DEFAULT cs16,

 rohc-ProfilesUL-Only-r15 SEQUENCE {

 profile0x0006-r15 BOOLEAN

 },

 rohc-ContextContinue-r15 ENUMERATED {supported} OPTIONAL,

 outOfOrderDelivery-r15 ENUMERATED {supported} OPTIONAL,

 sn-SizeLo-r15 ENUMERATED {supported} OPTIONAL,

 ims-VoiceOverNR-PDCP-MCG-Bearer-r15 ENUMERATED {supported} OPTIONAL,

 ims-VoiceOverNR-PDCP-SCG-Bearer-r15 ENUMERATED {supported} OPTIONAL

}

PDCP-ParametersNR-v1560 ::= SEQUENCE {

 ims-VoNR-PDCP-SCG-NGENDC-r15 ENUMERATED {supported} OPTIONAL

}

ROHC-ProfileSupportList-r15 ::= SEQUENCE {

 profile0x0001-r15 BOOLEAN,

 profile0x0002-r15 BOOLEAN,

 profile0x0003-r15 BOOLEAN,

 profile0x0004-r15 BOOLEAN,

 profile0x0006-r15 BOOLEAN,

 profile0x0101-r15 BOOLEAN,

 profile0x0102-r15 BOOLEAN,

 profile0x0103-r15 BOOLEAN,

 profile0x0104-r15 BOOLEAN

}

SupportedBandListNR-r15 ::= SEQUENCE (SIZE (1..maxBandsNR-r15)) OF SupportedBandNR-r15

SupportedBandNR-r15 ::= SEQUENCE {

 bandNR-r15 FreqBandIndicatorNR-r15

}

IRAT-ParametersUTRA-FDD ::= SEQUENCE {

 supportedBandListUTRA-FDD SupportedBandListUTRA-FDD

}

IRAT-ParametersUTRA-v920 ::= SEQUENCE {

 e-RedirectionUTRA-r9 ENUMERATED {supported}

}

IRAT-ParametersUTRA-v9c0 ::= SEQUENCE {

 voiceOverPS-HS-UTRA-FDD-r9 ENUMERATED {supported} OPTIONAL,

 voiceOverPS-HS-UTRA-TDD128-r9 ENUMERATED {supported} OPTIONAL,

 srvcc-FromUTRA-FDD-ToUTRA-FDD-r9 ENUMERATED {supported} OPTIONAL,

 srvcc-FromUTRA-FDD-ToGERAN-r9 ENUMERATED {supported} OPTIONAL,

 srvcc-FromUTRA-TDD128-ToUTRA-TDD128-r9 ENUMERATED {supported} OPTIONAL,

 srvcc-FromUTRA-TDD128-ToGERAN-r9 ENUMERATED {supported} OPTIONAL

}

IRAT-ParametersUTRA-v9h0 ::= SEQUENCE {

 mfbi-UTRA-r9 ENUMERATED {supported}

}

SupportedBandListUTRA-FDD ::= SEQUENCE (SIZE (1..maxBands)) OF SupportedBandUTRA-FDD

SupportedBandUTRA-FDD ::= ENUMERATED {

 bandI, bandII, bandIII, bandIV, bandV, bandVI,

 bandVII, bandVIII, bandIX, bandX, bandXI,

 bandXII, bandXIII, bandXIV, bandXV, bandXVI, ...,

 bandXVII-8a0, bandXVIII-8a0, bandXIX-8a0, bandXX-8a0,

 bandXXI-8a0, bandXXII-8a0, bandXXIII-8a0, bandXXIV-8a0,

 bandXXV-8a0, bandXXVI-8a0, bandXXVII-8a0, bandXXVIII-8a0,

 bandXXIX-8a0, bandXXX-8a0, bandXXXI-8a0, bandXXXII-8a0}

IRAT-ParametersUTRA-TDD128 ::= SEQUENCE {

 supportedBandListUTRA-TDD128 SupportedBandListUTRA-TDD128

}

SupportedBandListUTRA-TDD128 ::= SEQUENCE (SIZE (1..maxBands)) OF SupportedBandUTRA-TDD128

SupportedBandUTRA-TDD128 ::= ENUMERATED {

 a, b, c, d, e, f, g, h, i, j, k, l, m, n,

 o, p, ...}

IRAT-ParametersUTRA-TDD384 ::= SEQUENCE {

 supportedBandListUTRA-TDD384 SupportedBandListUTRA-TDD384

}

SupportedBandListUTRA-TDD384 ::= SEQUENCE (SIZE (1..maxBands)) OF SupportedBandUTRA-TDD384

SupportedBandUTRA-TDD384 ::= ENUMERATED {

 a, b, c, d, e, f, g, h, i, j, k, l, m, n,

 o, p, ...}

IRAT-ParametersUTRA-TDD768 ::= SEQUENCE {

 supportedBandListUTRA-TDD768 SupportedBandListUTRA-TDD768

}

SupportedBandListUTRA-TDD768 ::= SEQUENCE (SIZE (1..maxBands)) OF SupportedBandUTRA-TDD768

SupportedBandUTRA-TDD768 ::= ENUMERATED {

 a, b, c, d, e, f, g, h, i, j, k, l, m, n,

 o, p, ...}

IRAT-ParametersUTRA-TDD-v1020 ::= SEQUENCE {

 e-RedirectionUTRA-TDD-r10 ENUMERATED {supported}

}

IRAT-ParametersGERAN ::= SEQUENCE {

 supportedBandListGERAN SupportedBandListGERAN,

 interRAT-PS-HO-ToGERAN BOOLEAN

}

IRAT-ParametersGERAN-v920 ::= SEQUENCE {

 dtm-r9 ENUMERATED {supported} OPTIONAL,

 e-RedirectionGERAN-r9 ENUMERATED {supported} OPTIONAL

}

SupportedBandListGERAN ::= SEQUENCE (SIZE (1..maxBands)) OF SupportedBandGERAN

SupportedBandGERAN ::= ENUMERATED {

 gsm450, gsm480, gsm710, gsm750, gsm810, gsm850,

 gsm900P, gsm900E, gsm900R, gsm1800, gsm1900,

 spare5, spare4, spare3, spare2, spare1, ...}

IRAT-ParametersCDMA2000-HRPD ::= SEQUENCE {

 supportedBandListHRPD SupportedBandListHRPD,

 tx-ConfigHRPD ENUMERATED {single, dual},

 rx-ConfigHRPD ENUMERATED {single, dual}

}

SupportedBandListHRPD ::= SEQUENCE (SIZE (1..maxCDMA-BandClass)) OF BandclassCDMA2000

IRAT-ParametersCDMA2000-1XRTT ::= SEQUENCE {

 supportedBandList1XRTT SupportedBandList1XRTT,

 tx-Config1XRTT ENUMERATED {single, dual},

 rx-Config1XRTT ENUMERATED {single, dual}

}

IRAT-ParametersCDMA2000-1XRTT-v920 ::= SEQUENCE {

 e-CSFB-1XRTT-r9 ENUMERATED {supported},

 e-CSFB-ConcPS-Mob1XRTT-r9 ENUMERATED {supported} OPTIONAL

}

IRAT-ParametersCDMA2000-1XRTT-v1020 ::= SEQUENCE {

 e-CSFB-dual-1XRTT-r10 ENUMERATED {supported}

}

IRAT-ParametersCDMA2000-v1130 ::= SEQUENCE {

 cdma2000-NW-Sharing-r11 ENUMERATED {supported} OPTIONAL

}

SupportedBandList1XRTT ::= SEQUENCE (SIZE (1..maxCDMA-BandClass)) OF BandclassCDMA2000

IRAT-ParametersWLAN-r13 ::= SEQUENCE {

 supportedBandListWLAN-r13 SEQUENCE (SIZE (1..maxWLAN-Bands-r13)) OF WLAN-BandIndicator-r13 OPTIONAL

}

CSG-ProximityIndicationParameters-r9 ::= SEQUENCE {

 intraFreqProximityIndication-r9 ENUMERATED {supported} OPTIONAL,

 interFreqProximityIndication-r9 ENUMERATED {supported} OPTIONAL,

 utran-ProximityIndication-r9 ENUMERATED {supported} OPTIONAL

}

NeighCellSI-AcquisitionParameters-r9 ::= SEQUENCE {

 intraFreqSI-AcquisitionForHO-r9 ENUMERATED {supported} OPTIONAL,

 interFreqSI-AcquisitionForHO-r9 ENUMERATED {supported} OPTIONAL,

 utran-SI-AcquisitionForHO-r9 ENUMERATED {supported} OPTIONAL

}

NeighCellSI-AcquisitionParameters-v1530 ::= SEQUENCE {

 reportCGI-NR-EN-DC-r15 ENUMERATED {supported} OPTIONAL,

 reportCGI-NR-NoEN-DC-r15 ENUMERATED {supported} OPTIONAL

}

NeighCellSI-AcquisitionParameters-v1550 ::= SEQUENCE {

 eutra-CGI-Reporting-ENDC-r15 ENUMERATED {supported} OPTIONAL,

 utra-GERAN-CGI-Reporting-ENDC-r15 ENUMERATED {supported} OPTIONAL

}

NeighCellSI-AcquisitionParameters-v15a0 ::= SEQUENCE {

 eutra-CGI-Reporting-NEDC-r15 ENUMERATED {supported} OPTIONAL

}

NeighCellSI-AcquisitionParameters-v1610 ::= SEQUENCE {

 eutra-SI-AcquisitionForHO-ENDC-r16 ENUMERATED {supported} OPTIONAL,

 nr-AutonomousGaps-ENDC-FR1-r16 ENUMERATED {supported} OPTIONAL,

 nr-AutonomousGaps-ENDC-FR2-r16 ENUMERATED {supported} OPTIONAL,

 nr-AutonomousGaps-FR1-r16 ENUMERATED {supported} OPTIONAL,

 nr-AutonomousGaps-FR2-r16 ENUMERATED {supported} OPTIONAL

}

NeighCellSI-AcquisitionParameters-v1710 ::= SEQUENCE {

 gNB-ID-Length-Reporting-NR-EN-DC-r17 ENUMERATED {supported} OPTIONAL,

 gNB-ID-Length-Reporting-NR-NoEN-DC-r17 ENUMERATED {supported} OPTIONAL

}

SON-Parameters-r9 ::= SEQUENCE {

 rach-Report-r9 ENUMERATED {supported} OPTIONAL

}

SON-Parameters-v1800 ::= SEQUENCE {

 rach-ReportForNR-r18 ENUMERATED {supported} OPTIONAL

}

PUR-Parameters-r16 ::= SEQUENCE {

 pur-CP-5GC-CE-ModeA-r16 ENUMERATED {supported} OPTIONAL,

 pur-CP-5GC-CE-ModeB-r16 ENUMERATED {supported} OPTIONAL,

 pur-UP-5GC-CE-ModeA-r16 ENUMERATED {supported} OPTIONAL,

 pur-UP-5GC-CE-ModeB-r16 ENUMERATED {supported} OPTIONAL,

 pur-CP-EPC-CE-ModeA-r16 ENUMERATED {supported} OPTIONAL,

 pur-CP-EPC-CE-ModeB-r16 ENUMERATED {supported} OPTIONAL,

 pur-UP-EPC-CE-ModeA-r16 ENUMERATED {supported} OPTIONAL,

 pur-UP-EPC-CE-ModeB-r16 ENUMERATED {supported} OPTIONAL,

 pur-CP-L1Ack-r16 ENUMERATED {supported} OPTIONAL,

 pur-FrequencyHopping-r16 ENUMERATED {supported} OPTIONAL,

 pur-PUSCH-NB-MaxTBS-r16 ENUMERATED {supported} OPTIONAL,

 pur-RSRP-Validation-r16 ENUMERATED {supported} OPTIONAL,

 pur-SubPRB-CE-ModeA-r16 ENUMERATED {supported} OPTIONAL,

 pur-SubPRB-CE-ModeB-r16 ENUMERATED {supported} OPTIONAL

}

UE-BasedNetwPerfMeasParameters-r10 ::= SEQUENCE {

 loggedMeasurementsIdle-r10 ENUMERATED {supported} OPTIONAL,

 standaloneGNSS-Location-r10 ENUMERATED {supported} OPTIONAL

}

UE-BasedNetwPerfMeasParameters-v1250 ::= SEQUENCE {

 loggedMBSFNMeasurements-r12 ENUMERATED {supported}

}

UE-BasedNetwPerfMeasParameters-v1430 ::= SEQUENCE {

 locationReport-r14 ENUMERATED {supported} OPTIONAL

}

UE-BasedNetwPerfMeasParameters-v1530 ::= SEQUENCE {

 loggedMeasBT-r15 ENUMERATED {supported} OPTIONAL,

 loggedMeasWLAN-r15 ENUMERATED {supported} OPTIONAL,

 immMeasBT-r15 ENUMERATED {supported} OPTIONAL,

 immMeasWLAN-r15 ENUMERATED {supported} OPTIONAL

}

UE-BasedNetwPerfMeasParameters-v1610 ::= SEQUENCE {

 ul-PDCP-AvgDelay-r16 ENUMERATED {supported} OPTIONAL

}

UE-BasedNetwPerfMeasParameters-v1700 ::= SEQUENCE {

 loggedMeasIdleEventL1-r17 ENUMERATED {supported} OPTIONAL,

 loggedMeasIdleEventOutOfCoverage-r17 ENUMERATED {supported} OPTIONAL,

 loggedMeasUncomBarPre-r17 ENUMERATED {supported} OPTIONAL,

 immMeasUncomBarPre-r17 ENUMERATED {supported} OPTIONAL

}

UE-BasedNetwPerfMeasParameters-v1800 ::= SEQUENCE {

 sigBasedEUTRA-LoggedMeasOverrideProtect-r18 ENUMERATED {supported} OPTIONAL

}

OTDOA-PositioningCapabilities-r10 ::= SEQUENCE {

 otdoa-UE-Assisted-r10 ENUMERATED {supported},

 interFreqRSTD-Measurement-r10 ENUMERATED {supported} OPTIONAL

}

Other-Parameters-r11 ::= SEQUENCE {

 inDeviceCoexInd-r11 ENUMERATED {supported} OPTIONAL,

 powerPrefInd-r11 ENUMERATED {supported} OPTIONAL,

 ue-Rx-TxTimeDiffMeasurements-r11 ENUMERATED {supported} OPTIONAL

}

Other-Parameters-v11d0 ::= SEQUENCE {

 inDeviceCoexInd-UL-CA-r11 ENUMERATED {supported} OPTIONAL

}

Other-Parameters-v1360 ::= SEQUENCE {

 inDeviceCoexInd-HardwareSharingInd-r13 ENUMERATED {supported} OPTIONAL

}

Other-Parameters-v1430 ::= SEQUENCE {

 bwPrefInd-r14 ENUMERATED {supported} OPTIONAL,

 rlm-ReportSupport-r14 ENUMERATED {supported} OPTIONAL

}

OtherParameters-v1450 ::= SEQUENCE {

 overheatingInd-r14 ENUMERATED {supported} OPTIONAL

}

Other-Parameters-v1460 ::= SEQUENCE {

 nonCSG-SI-Reporting-r14 ENUMERATED {supported} OPTIONAL

}

Other-Parameters-v1530 ::= SEQUENCE {

 assistInfoBitForLC-r15 ENUMERATED {supported} OPTIONAL,

 timeReferenceProvision-r15 ENUMERATED {supported} OPTIONAL,

 flightPathPlan-r15 ENUMERATED {supported} OPTIONAL

}

Other-Parameters-v1540 ::= SEQUENCE {

 inDeviceCoexInd-ENDC-r15 ENUMERATED {supported} OPTIONAL

}

Other-Parameters-v1610 ::= SEQUENCE {

 resumeWithStoredMCG-SCells-r16 ENUMERATED {supported} OPTIONAL,

 resumeWithMCG-SCellConfig-r16 ENUMERATED {supported} OPTIONAL,

 resumeWithStoredSCG-r16 ENUMERATED {supported} OPTIONAL,

 resumeWithSCG-Config-r16 ENUMERATED {supported} OPTIONAL,

 mcgRLF-RecoveryViaSCG-r16 ENUMERATED {supported} OPTIONAL,

 overheatingIndForSCG-r16 ENUMERATED {supported} OPTIONAL

}

Other-Parameters-v1650 ::= SEQUENCE {

 mpsPriorityIndication-r16 ENUMERATED {supported} OPTIONAL

}

Other-Parameters-v1690 ::= SEQUENCE {

 ul-RRC-Segmentation-r16 ENUMERATED {supported} OPTIONAL

}

MBMS-Parameters-r11 ::= SEQUENCE {

 mbms-SCell-r11 ENUMERATED {supported} OPTIONAL,

 mbms-NonServingCell-r11 ENUMERATED {supported} OPTIONAL

}

MBMS-Parameters-v1250 ::= SEQUENCE {

 mbms-AsyncDC-r12 ENUMERATED {supported} OPTIONAL

}

MBMS-Parameters-v1430 ::= SEQUENCE {

 fembmsDedicatedCell-r14 ENUMERATED {supported} OPTIONAL,

 fembmsMixedCell-r14 ENUMERATED {supported} OPTIONAL,

 subcarrierSpacingMBMS-khz7dot5-r14 ENUMERATED {supported} OPTIONAL,

 subcarrierSpacingMBMS-khz1dot25-r14 ENUMERATED {supported} OPTIONAL

}

MBMS-Parameters-v1470 ::= SEQUENCE {

 mbms-MaxBW-r14 CHOICE {

 implicitValue NULL,

 explicitValue INTEGER(2..20)

 },

 mbms-ScalingFactor1dot25-r14 ENUMERATED {n3, n6, n9, n12} OPTIONAL,

 mbms-ScalingFactor7dot5-r14 ENUMERATED {n1, n2, n3, n4} OPTIONAL

}

MBMS-Parameters-v1610 ::= SEQUENCE {

 mbms-ScalingFactor2dot5-r16 ENUMERATED {n2, n4, n6, n8} OPTIONAL,

 mbms-ScalingFactor0dot37-r16 ENUMERATED {n12, n16, n20, n24} OPTIONAL,

 mbms-SupportedBandInfoList-r16 SEQUENCE (SIZE (1..maxBands)) OF MBMS-SupportedBandInfo-r16

}

MBMS-Parameters-v1700 ::= SEQUENCE {

 mbms-SupportedBandInfoList-v1700 SEQUENCE (SIZE (1..maxBands)) OF MBMS-SupportedBandInfo-v1700 OPTIONAL

}

MBMS-SupportedBandInfo-r16 ::= SEQUENCE {

 subcarrierSpacingMBMS-khz2dot5-r16 ENUMERATED {supported} OPTIONAL,

 subcarrierSpacingMBMS-khz0dot37-r16 SEQUENCE {

 timeSeparationSlot2-r16 ENUMERATED {supported} OPTIONAL,

 timeSeparationSlot4-r16 ENUMERATED {supported} OPTIONAL

 } OPTIONAL

}

MBMS-SupportedBandInfo-v1700 ::= SEQUENCE {

 pmch-Bandwidth-n40-r17 ENUMERATED {supported} OPTIONAL,

 pmch-Bandwidth-n35-r17 ENUMERATED {supported} OPTIONAL,

 pmch-Bandwidth-n30-r17 ENUMERATED {supported} OPTIONAL

}

FeMBMS-Unicast-Parameters-r14 ::= SEQUENCE {

 unicast-fembmsMixedSCell-r14 ENUMERATED {supported} OPTIONAL,

 emptyUnicastRegion-r14 ENUMERATED {supported} OPTIONAL

}

SCPTM-Parameters-r13 ::= SEQUENCE {

 scptm-ParallelReception-r13 ENUMERATED {supported} OPTIONAL,

 scptm-SCell-r13 ENUMERATED {supported} OPTIONAL,

 scptm-NonServingCell-r13 ENUMERATED {supported} OPTIONAL,

 scptm-AsyncDC-r13 ENUMERATED {supported} OPTIONAL

}

CE-Parameters-r13 ::= SEQUENCE {

 ce-ModeA-r13 ENUMERATED {supported} OPTIONAL,

 ce-ModeB-r13 ENUMERATED {supported} OPTIONAL

}

CE-Parameters-v1320 ::= SEQUENCE {

 intraFreqA3-CE-ModeA-r13 ENUMERATED {supported} OPTIONAL,

 intraFreqA3-CE-ModeB-r13 ENUMERATED {supported} OPTIONAL,

 intraFreqHO-CE-ModeA-r13 ENUMERATED {supported} OPTIONAL,

 intraFreqHO-CE-ModeB-r13 ENUMERATED {supported} OPTIONAL

}

CE-Parameters-v1350 ::= SEQUENCE {

 unicastFrequencyHopping-r13 ENUMERATED {supported} OPTIONAL

}

CE-Parameters-v1370 ::= SEQUENCE {

 tm9-CE-ModeA-r13 ENUMERATED {supported} OPTIONAL,

 tm9-CE-ModeB-r13 ENUMERATED {supported} OPTIONAL

}

CE-Parameters-v1380 ::= SEQUENCE {

 tm6-CE-ModeA-r13 ENUMERATED {supported} OPTIONAL

}

CE-Parameters-v1430 ::= SEQUENCE {

 ce-SwitchWithoutHO-r14 ENUMERATED {supported} OPTIONAL

}

CE-MultiTB-Parameters-r16 ::= SEQUENCE {

 pdsch-MultiTB-CE-ModeA-r16 ENUMERATED {supported} OPTIONAL,

 pdsch-MultiTB-CE-ModeB-r16 ENUMERATED {supported} OPTIONAL,

 pusch-MultiTB-CE-ModeA-r16 ENUMERATED {supported} OPTIONAL,

 pusch-MultiTB-CE-ModeB-r16 ENUMERATED {supported} OPTIONAL,

 ce-MultiTB-64QAM-r16 ENUMERATED {supported} OPTIONAL,

 ce-MultiTB-EarlyTermination-r16 ENUMERATED {supported} OPTIONAL,

 ce-MultiTB-FrequencyHopping-r16 ENUMERATED {supported} OPTIONAL,

 ce-MultiTB-HARQ-AckBundling-r16 ENUMERATED {supported} OPTIONAL,

 ce-MultiTB-Interleaving-r16 ENUMERATED {supported} OPTIONAL,

 ce-MultiTB-SubPRB-r16 ENUMERATED {supported} OPTIONAL

}

CE-ResourceResvParameters-r16 ::= SEQUENCE {

 subframeResourceResvDL-CE-ModeA-r16 ENUMERATED {supported} OPTIONAL,

 subframeResourceResvDL-CE-ModeB-r16 ENUMERATED {supported} OPTIONAL,

 subframeResourceResvUL-CE-ModeA-r16 ENUMERATED {supported} OPTIONAL,

 subframeResourceResvUL-CE-ModeB-r16 ENUMERATED {supported} OPTIONAL,

 slotSymbolResourceResvDL-CE-ModeA-r16 ENUMERATED {supported} OPTIONAL,

 slotSymbolResourceResvDL-CE-ModeB-r16 ENUMERATED {supported} OPTIONAL,

 slotSymbolResourceResvUL-CE-ModeA-r16 ENUMERATED {supported} OPTIONAL,

 slotSymbolResourceResvUL-CE-ModeB-r16 ENUMERATED {supported} OPTIONAL,

 subcarrierPuncturingCE-ModeA-r16 ENUMERATED {supported} OPTIONAL,

 subcarrierPuncturingCE-ModeB-r16 ENUMERATED {supported} OPTIONAL

}

LAA-Parameters-r13 ::= SEQUENCE {

 crossCarrierSchedulingLAA-DL-r13 ENUMERATED {supported} OPTIONAL,

 csi-RS-DRS-RRM-MeasurementsLAA-r13 ENUMERATED {supported} OPTIONAL,

 downlinkLAA-r13 ENUMERATED {supported} OPTIONAL,

 endingDwPTS-r13 ENUMERATED {supported} OPTIONAL,

 secondSlotStartingPosition-r13 ENUMERATED {supported} OPTIONAL,

 tm9-LAA-r13 ENUMERATED {supported} OPTIONAL,

 tm10-LAA-r13 ENUMERATED {supported} OPTIONAL

}

LAA-Parameters-v1430 ::= SEQUENCE {

 crossCarrierSchedulingLAA-UL-r14 ENUMERATED {supported} OPTIONAL,

 uplinkLAA-r14 ENUMERATED {supported} OPTIONAL,

 twoStepSchedulingTimingInfo-r14 ENUMERATED {nPlus1, nPlus2, nPlus3} OPTIONAL,

 uss-BlindDecodingAdjustment-r14 ENUMERATED {supported} OPTIONAL,

 uss-BlindDecodingReduction-r14 ENUMERATED {supported} OPTIONAL,

 outOfSequenceGrantHandling-r14 ENUMERATED {supported} OPTIONAL

}

LAA-Parameters-v1530 ::= SEQUENCE {

 aul-r15 ENUMERATED {supported} OPTIONAL,

 laa-PUSCH-Mode1-r15 ENUMERATED {supported} OPTIONAL,

 laa-PUSCH-Mode2-r15 ENUMERATED {supported} OPTIONAL,

 laa-PUSCH-Mode3-r15 ENUMERATED {supported} OPTIONAL

}

WLAN-IW-Parameters-r12 ::= SEQUENCE {

 wlan-IW-RAN-Rules-r12 ENUMERATED {supported} OPTIONAL,

 wlan-IW-ANDSF-Policies-r12 ENUMERATED {supported} OPTIONAL

}

LWA-Parameters-r13 ::= SEQUENCE {

 lwa-r13 ENUMERATED {supported} OPTIONAL,

 lwa-SplitBearer-r13 ENUMERATED {supported} OPTIONAL,

 wlan-MAC-Address-r13 OCTET STRING (SIZE (6)) OPTIONAL,

 lwa-BufferSize-r13 ENUMERATED {supported} OPTIONAL

}

LWA-Parameters-v1430 ::= SEQUENCE {

 lwa-HO-WithoutWT-Change-r14 ENUMERATED {supported} OPTIONAL,

 lwa-UL-r14 ENUMERATED {supported} OPTIONAL,

 wlan-PeriodicMeas-r14 ENUMERATED {supported} OPTIONAL,

 wlan-ReportAnyWLAN-r14 ENUMERATED {supported} OPTIONAL,

 wlan-SupportedDataRate-r14 INTEGER (1..2048) OPTIONAL

}

LWA-Parameters-v1440 ::= SEQUENCE {

 lwa-RLC-UM-r14 ENUMERATED {supported} OPTIONAL

}

WLAN-IW-Parameters-v1310 ::= SEQUENCE {

 rclwi-r13 ENUMERATED {supported} OPTIONAL

}

LWIP-Parameters-r13 ::= SEQUENCE {

 lwip-r13 ENUMERATED {supported} OPTIONAL

}

LWIP-Parameters-v1430 ::= SEQUENCE {

 lwip-Aggregation-DL-r14 ENUMERATED {supported} OPTIONAL,

 lwip-Aggregation-UL-r14 ENUMERATED {supported} OPTIONAL

}

NAICS-Capability-List-r12 ::= SEQUENCE (SIZE (1..maxNAICS-Entries-r12)) OF NAICS-Capability-Entry-r12

NAICS-Capability-Entry-r12 ::= SEQUENCE {

 numberOfNAICS-CapableCC-r12 INTEGER(1..5),

 numberOfAggregatedPRB-r12 ENUMERATED {

 n50, n75, n100, n125, n150, n175,

 n200, n225, n250, n275, n300, n350,

 n400, n450, n500, spare},

 ...

}

SL-Parameters-r12 ::= SEQUENCE {

 commSimultaneousTx-r12 ENUMERATED {supported} OPTIONAL,

 commSupportedBands-r12 FreqBandIndicatorListEUTRA-r12 OPTIONAL,

 discSupportedBands-r12 SupportedBandInfoList-r12 OPTIONAL,

 discScheduledResourceAlloc-r12 ENUMERATED {supported} OPTIONAL,

 disc-UE-SelectedResourceAlloc-r12 ENUMERATED {supported} OPTIONAL,

 disc-SLSS-r12 ENUMERATED {supported} OPTIONAL,

 discSupportedProc-r12 ENUMERATED {n50, n400} OPTIONAL

}

SL-Parameters-v1310 ::= SEQUENCE {

 discSysInfoReporting-r13 ENUMERATED {supported} OPTIONAL,

 commMultipleTx-r13 ENUMERATED {supported} OPTIONAL,

 discInterFreqTx-r13 ENUMERATED {supported} OPTIONAL,

 discPeriodicSLSS-r13 ENUMERATED {supported} OPTIONAL

}

SL-Parameters-v1430 ::= SEQUENCE {

 zoneBasedPoolSelection-r14 ENUMERATED {supported} OPTIONAL,

 ue-AutonomousWithFullSensing-r14 ENUMERATED {supported} OPTIONAL,

 ue-AutonomousWithPartialSensing-r14 ENUMERATED {supported} OPTIONAL,

 sl-CongestionControl-r14 ENUMERATED {supported} OPTIONAL,

 v2x-TxWithShortResvInterval-r14 ENUMERATED {supported} OPTIONAL,

 v2x-numberTxRxTiming-r14 INTEGER(1..16) OPTIONAL,

 v2x-nonAdjacentPSCCH-PSSCH-r14 ENUMERATED {supported} OPTIONAL,

 slss-TxRx-r14 ENUMERATED {supported} OPTIONAL,

 v2x-SupportedBandCombinationList-r14 V2X-SupportedBandCombination-r14 OPTIONAL

}

SL-Parameters-v1530 ::= SEQUENCE {

 slss-SupportedTxFreq-r15 ENUMERATED {single, multiple} OPTIONAL,

 sl-64QAM-Tx-r15 ENUMERATED {supported} OPTIONAL,

 sl-TxDiversity-r15 ENUMERATED {supported} OPTIONAL,

 ue-CategorySL-r15 UE-CategorySL-r15 OPTIONAL,

 v2x-SupportedBandCombinationList-v1530 V2X-SupportedBandCombination-v1530 OPTIONAL

}

SL-Parameters-v1540 ::= SEQUENCE {

 sl-64QAM-Rx-r15 ENUMERATED {supported} OPTIONAL,

 sl-RateMatchingTBSScaling-r15 ENUMERATED {supported} OPTIONAL,

 sl-LowT2min-r15 ENUMERATED {supported} OPTIONAL,

 v2x-SensingReportingMode3-r15 ENUMERATED {supported} OPTIONAL

}

SL-Parameters-v1610 ::= SEQUENCE {

 sl-ParameterNR-r16 OCTET STRING OPTIONAL,

 dummy V2X-SupportedBandCombinationEUTRA-NR-r16 OPTIONAL

}

SL-Parameters-v1630 ::= SEQUENCE {

 v2x-SupportedBandCombinationListEUTRA-NR-r16 V2X-SupportedBandCombinationEUTRA-NR-v1630 OPTIONAL

}

SL-Parameters-v1710 ::= SEQUENCE {

 v2x-SupportedBandCombinationListEUTRA-NR-v1710 V2X-SupportedBandCombinationEUTRA-NR-v1710 OPTIONAL

}

SL-Parameters-v1800 ::= SEQUENCE {

 sl-A2X-SupportedBandCombinationList-r18 SL-A2X-SupportedBandCombination-r18 OPTIONAL,

 sl-A2X-Service-r18 ENUMERATED {brid, daa, bridAndDAA} OPTIONAL

}

UE-CategorySL-r15 ::= SEQUENCE {

 ue-CategorySL-C-TX-r15 INTEGER(1..5),

 ue-CategorySL-C-RX-r15 INTEGER(1..4)

}

V2X-SupportedBandCombination-r14 ::= SEQUENCE (SIZE (1..maxBandComb-r13)) OF V2X-BandCombinationParameters-r14

V2X-SupportedBandCombination-v1530 ::= SEQUENCE (SIZE (1..maxBandComb-r13)) OF V2X-BandCombinationParameters-v1530

V2X-BandCombinationParameters-r14 ::= SEQUENCE (SIZE (1.. maxSimultaneousBands-r10)) OF V2X-BandParameters-r14

V2X-BandCombinationParameters-v1530 ::= SEQUENCE (SIZE (1.. maxSimultaneousBands-r10)) OF V2X-BandParameters-v1530

V2X-SupportedBandCombinationEUTRA-NR-r16 ::= SEQUENCE (SIZE (1..maxBandCombSidelinkNR-r16)) OF V2X-BandParametersEUTRA-NR-r16

V2X-SupportedBandCombinationEUTRA-NR-v1630 ::= SEQUENCE (SIZE (1..maxBandCombSidelinkNR-r16)) OF V2X-BandCombinationParametersEUTRA-NR-v1630

V2X-SupportedBandCombinationEUTRA-NR-v1710 ::= SEQUENCE (SIZE (1..maxBandCombSidelinkNR-r16)) OF V2X-BandCombinationParametersEUTRA-NR-v1710

V2X-BandCombinationParametersEUTRA-NR-v1630 ::= SEQUENCE {

 bandListSidelinkEUTRA-NR-r16 SEQUENCE (SIZE (1.. maxSimultaneousBands-r10)) OF V2X-BandParametersEUTRA-NR-r16,

 bandListSidelinkEUTRA-NR-v1630 SEQUENCE (SIZE (1.. maxSimultaneousBands-r10)) OF V2X-BandParametersEUTRA-NR-v1630

}

V2X-BandCombinationParametersEUTRA-NR-v1710 ::= SEQUENCE (SIZE (1..maxSimultaneousBands-r10)) OF V2X-BandParametersEUTRA-NR-v1710

V2X-BandParametersEUTRA-NR-r16 ::= CHOICE {

 eutra SEQUENCE {

 v2x-BandParameters1-r16 V2X-BandParameters-r14 OPTIONAL,

 v2x-BandParameters2-r16 V2X-BandParameters-v1530 OPTIONAL

 },

 nr SEQUENCE {

 v2x-BandParametersNR-r16 OCTET STRING OPTIONAL

 }

}

V2X-BandParametersEUTRA-NR-v1630 ::= CHOICE {

 eutra NULL,

 nr SEQUENCE {

 tx-Sidelink-r16 ENUMERATED {supported} OPTIONAL,

 rx-Sidelink-r16 ENUMERATED {supported} OPTIONAL

 }

}

V2X-BandParametersEUTRA-NR-v1710 ::= SEQUENCE {

 v2x-BandParametersEUTRA-NR-v1710 OCTET STRING OPTIONAL

}

SL-A2X-SupportedBandCombination-r18 ::= SEQUENCE (SIZE (1..maxBandComb-r13)) OF SL-A2X-BandCombinationParameters-r18

SL-A2X-BandCombinationParameters-r18 ::= SEQUENCE (SIZE (1.. maxSimultaneousBands-r10)) OF SL-A2X-BandParameters-r18

SL-A2X-BandParameters-r18 ::= SEQUENCE {

 a2x-FreqBandEUTRA-r18 FreqBandIndicator-r11,

 a2x-BandParametersTxSL-r18 BandParametersTxA2X-r18 OPTIONAL,

 a2x-BandParametersRxSL-r18 BandParametersRxA2X-r18 OPTIONAL

}

BandParametersTxA2X-r18 ::= SEQUENCE {

 a2x-BandwidthClassTxSL-r18 V2X-BandwidthClassSL-r14

}

BandParametersRxA2X-r18 ::= SEQUENCE {

 a2x-BandwidthClassRxSL-r18 V2X-BandwidthClassSL-r14

}

SupportedBandInfoList-r12 ::= SEQUENCE (SIZE (1..maxBands)) OF SupportedBandInfo-r12

SupportedBandInfo-r12 ::= SEQUENCE {

 support-r12 ENUMERATED {supported} OPTIONAL

}

FreqBandIndicatorListEUTRA-r12 ::= SEQUENCE (SIZE (1..maxBands)) OF FreqBandIndicator-r11

MMTEL-Parameters-r14 ::= SEQUENCE {

 delayBudgetReporting-r14 ENUMERATED {supported} OPTIONAL,

 pusch-Enhancements-r14 ENUMERATED {supported} OPTIONAL,

 recommendedBitRate-r14 ENUMERATED {supported} OPTIONAL,

 recommendedBitRateQuery-r14 ENUMERATED {supported} OPTIONAL

}

MMTEL-Parameters-v1610 ::= SEQUENCE {

 recommendedBitRateMultiplier-r16 ENUMERATED {supported} OPTIONAL

}

SRS-CapabilityPerBandPair-r14 ::= SEQUENCE {

 retuningInfo SEQUENCE {

 rf-RetuningTimeDL-r14 ENUMERATED {n0, n0dot5, n1, n1dot5, n2, n2dot5, n3,

 n3dot5, n4, n4dot5, n5, n5dot5, n6, n6dot5,

 n7, spare1} OPTIONAL,

 rf-RetuningTimeUL-r14 ENUMERATED {n0, n0dot5, n1, n1dot5, n2, n2dot5, n3,

 n3dot5, n4, n4dot5, n5, n5dot5, n6, n6dot5,

 n7, spare1} OPTIONAL

 }

}

SRS-CapabilityPerBandPair-v14b0 ::= SEQUENCE {

 srs-FlexibleTiming-r14 ENUMERATED {supported} OPTIONAL,

 srs-HARQ-ReferenceConfig-r14 ENUMERATED {supported} OPTIONAL

}

SRS-CapabilityPerBandPair-v1610::= SEQUENCE {

 addSRS-CarrierSwitching-r16 ENUMERATED {supported} OPTIONAL

}

HighSpeedEnhParameters-r14 ::= SEQUENCE {

 measurementEnhancements-r14 ENUMERATED {supported} OPTIONAL,

 demodulationEnhancements-r14 ENUMERATED {supported} OPTIONAL,

 prach-Enhancements-r14 ENUMERATED {supported} OPTIONAL

}

HighSpeedEnhParameters-v1610 ::= SEQUENCE {

 measurementEnhancementsSCell-r16 ENUMERATED {supported} OPTIONAL,

 measurementEnhancements2-r16 ENUMERATED {supported} OPTIONAL,

 demodulationEnhancements2-r16 ENUMERATED {supported} OPTIONAL,

 interRAT-enhancementNR-r16 ENUMERATED {supported} OPTIONAL

}

-- ASN1STOP

| *UE-EUTRA-Capability* field descriptions | *FDD/ TDD diff* |
| --- | --- |
| ***accessStratumRelease***This field indicates the release supported by the UE. NOTE 7. | - |
| ***additionalRx-Tx-PerformanceReq***Indicates whether the UE supports the additional Rx and Tx performance requirement for a given band combination as specified in TS 36.101 [42]. | - |
| ***addSRS***Presence of this field indicates the UE supports the additional SRS symbol(s) within the normal UL subframes in TDD as described in TS 36.213 [23].  | - |
| ***addSRS-1T2R***Indicates whether the UE supports selecting one antenna among two antennas to transmit additional SRS symbol(s) for the corresponding band of the band combination as described in TS 36.213 [23]. | - |
| ***addSRS-1T4R***Indicates whether the UE supports selecting one antenna among four antennas to transmit additional SRS symbol(s) for the corresponding band of the band combination as described in TS 36.213 [23]. | - |
| ***addSRS-2T4R-2Pairs***Indicates whether the UE supports selecting one antenna pair between two antenna pairs to transmit additional SRS symbol(s) simultaneously for the corresponding band of the band combination as described in TS 36.213 [23]. | - |
| ***addSRS-2T4R-3Pairs***Indicates whether the UE supports selecting one antenna pair among three antenna pairs to transmit additional SRS symbol(s) simultaneously for the corresponding band of the band combination as described in TS 36.213 [23]. | - |
| ***addSRS-AntennaSwitching (in addSRS)***Value *useBasic* indicates the antenna switching capabilities for additional SRS symbol(s) for a band of band combination for which the capability is not signalled in *bandParameterList-v1610* is the same as indicated by *bandParameterList-v1380* and/or *bandParameterList-v1530* for the concerned band of band combination.  | - |
| ***addSRS-AntennaSwitching (in bandParameterList-v1610)***If signalled, the field indicates the antenna switching capabilities for additional SRS symbol(s) for the concerned band of band combination. | - |
| ***addSRS-CarrierSwitching (in addSRS)***Indicates whether carrier switching is supported for additional SRS symbol(s) for all band pairs of band combinations for which UE supports SRS carrier switching. This field is included only if *srs-CapabilityPerBandPairList-r14* is included. If this field is included, *addSRS-CarrierSwitching* (in *bandParameterList-v1610*) is not included. | - |
| ***addSRS-CarrierSwitching (in bandParameterList-v1610)***Indicates whether carrier switching is supported for additional SRS symbol(s) for the concerned band pair of band combination. This field is included only if *srs-CapabilityPerBandPairList-r14* is included.If this field is included, *addSRS-CarrierSwitching* (in *addSRS*) is not included. | - |
| ***addSRS-FrequencyHopping (in addSRS)***Indicates whether frequency hopping is supported for additional SRS symbol(s) for all bands of band combinations for which the capability is not signalled in *bandParameterList-v1610*. | - |
| ***addSRS-FrequencyHopping (in bandParameterList-v1610)***If signalled, the field indicates whether frequency hopping is supported for additional SRS symbol(s) for the concerned band of band combination. | - |
| ***allowedCellList***Indicates whether the UE supports EUTRA allowed-cell listing to limit the set of cells applicable for measurements. | - |
| ***alternativeTBS-Indices***Indicates whether the UE supports alternative TBS indices *I*TBS 26A and 33A as specified in TS 36.213 [23]. | - |
| ***alternativeTBS-Index***Indicates whether the UE supports alternative TBS index ITBS 33B as specified in TS 36.213 [23]. | No |
| ***alternativeTimeToTrigger***Indicates whether the UE supports alternativeTimeToTrigger. | No |
| ***altFreqPriority***Indicates whether the UE supports alternative cell reselection priority. | No |
| ***altMCS-Table***Indicates whether the UE supports the 6-bit MCS table as specified in TS 36.212 [22] and TS 36.213 [23]. | Yes |
| ***aperiodicCSI-Reporting***Indicates whether the UE supports aperiodic CSI reporting with 3 bits of the CSI request field size as specified in TS 36.213 [23], clause 7.2.1 and/or aperiodic CSI reporting mode 1-0 and mode 1-1 as specified in TS 36.213 [23], clause 7.2.1. The first bit is set to "1" if the UE supports the aperiodic CSI reporting with 3 bits of the CSI request field size. The second bit is set to "1" if the UE supports the aperiodic CSI reporting mode 1-0 and mode 1-1. | No |
| ***aperiodicCsi-ReportingSTTI***Indicates whether the UE supports aperiodic CSI reporting for short TTI as specified in TS 36.213 [23], clause 7.2.1. | Yes |
| ***appliedCapabilityFilterCommon***Contains the filter, applied by the UE, common for all MR-DC related capability containers that are requested and as defined by *UE-CapabilityRequestFilterCommon* IE in TS 38.331 [82]. | - |
| ***assistInfoBitForLC***Indicates whether the UE supports assistance information bit for local cache. | - |
| ***aul***Indicates whether the UE supports AUL as specified n TS 36.321 [6]. | - |
| ***bandCombinationListEUTRA***One entry corresponding to each supported band combination listed in the same order as in *supportedBandCombination.*  | - |
| ***BandCombinationParameters-v1090, BandCombinationParameters-v10i0, BandCombinationParameters-v1270***If included, the UE shall include the same number of entries, and listed in the same order, as in *BandCombinationParameters-r10*. | - |
| ***BandCombinationParameters-v1130***The field is applicable to each supported CA bandwidth class combination (i.e. CA configuration in TS 36.101 [42], clause 5.6A.1) indicated in the corresponding band combination. If included, the UE shall include the same number of entries, and listed in the same order, as in *BandCombinationParameters-r10*. | - |
| ***bandEUTRA***E‑UTRA band as defined in TS 36.101 [42] and TS 36.102 [113] for NTN capable UE. In case the UE includes *bandEUTRA-v9e0* or *bandEUTRA-v1090*, the UE shall set the corresponding entry of *bandEUTRA* (i.e. without suffix) or *bandEUTRA-r10* respectively to *maxFBI*. | - |
| ***bandInfoNR-v1610, bandInfoNR-v1800***One entry corresponding to each supported E-UTRA band listed in the same order as in *supportedBandListEUTRA*. If *bandInfoNR-v1610* is absent, network assumes gap is required when measurement is performed on any NR bands while UE is served by cell(s) belongs to a E-UTRA band listed in *supportedBandListEUTRA* except for the FR2 inter-RAT measurement which depends on the support of *independentGapConfig*. | - |
| ***bandListEUTRA***One entry corresponding to each supported E‑UTRA band listed in the same order as in *supportedBandListEUTRA*. | - |
| ***bandParameterList-v1380***If included, the UE shall include the same number of entries listed in the same order as the band entries in the corresponding band combination. | - |
| ***bandParametersUL, bandParametersDL***Indicates the supported parameters for the band. Each of *CA-MIMO-ParametersUL* and *CA-MIMO-ParametersDL* can be included only once for one band in a single band combination entry. | - |
| ***beamformed (in MIMO-CA-ParametersPerBoBCPerTM)***If signalled, the field indicates for a particular transmission mode, the UE capabilities concerning beamformed EBF/ FD-MIMO operation (class B) applicable for the concerned band combination. | - |
| ***beamformed (in MIMO-UE-ParametersPerTM)***Indicates for a particular transmission mode, the UE capabilities concerning beamformed EBF/ FD-MIMO operation (class B) applicable for band combinations for which the concerned capabilities are not signalled. | Yes |
| ***benefitsFromInterruption***Indicates whether the UE power consumption would benefit from being allowed to cause interruptions to serving cells when performing measurements of deactivated SCell carriers for *measCycleSCell* of less than 640ms, as specified in TS 36.133 [16]. | No |
| ***bwPrefInd***Indicates whether the UE supports maximum PDSCH/PUSCH bandwidth preference indication. | - |
| ***ca-BandwidthClass***The CA bandwidth class supported by the UE as defined in TS 36.101 [42], Table 5.6A-1.The UE explicitly includes all the supported CA bandwidth class combinations in the band combination signalling. Support for one CA bandwidth class does not implicitly indicate support for another CA bandwidth class. | - |
| ***ca-IdleModeMeasurements***Indicates whether UE supports reporting measurements performed during RRC\_IDLE. | - |
| ***ca-IdleModeValidityArea***Indicates whether UE supports validity area for IDLE measurements during RRC\_IDLE. | - |
| ***cch-IM-RefRecTypeA-OneRX-Port***This field defines whether the DL Category 1bis or the DL Category M2 UE supports Type A downlink control channel interference mitigation (CCH-IM) receiver "LMMSE-IRC + CRS-IC" for PDCCH/PCFICH/PHICH/EPDCCH receive processing (Enhanced downlink control channel performance requirements Type A in TS 36.101 [6]). | No |
| ***cch-InterfMitigation-RefRecTypeA, cch-InterfMitigation-RefRecTypeB, cch-InterfMitigation-MaxNumCCs***The field *cch-InterfMitigation-RefRecTypeA* defines whether the UE supports Type A downlink control channel interference mitigation (CCH-IM) receiver "LMMSE-IRC + CRS-IC" for PDCCH/PCFICH/PHICH/EPDCCH receive processing (Enhanced downlink control channel performance requirements Type A in the TS 36.101 [6]). The field *cch-InterfMitigation-RefRecTypeB* defines whether the UE supports Type B downlink CCH-IM receiver "E-LMMSE-IRC + CRS-IC" for PDCCH/PCFICH/PHICH receive processing in synchronous networks (Enhanced downlink control channel performance requirements Type B in the TS 36.101 [6]). The UE supporting the capability defined by *cch-InterfMitigation-RefRecTypeB-r13* shall also support the capability defined by *cch-InterfMitigation-RefRecTypeA-r13*.If the UE sets one or more of the fields *cch-InterfMitigation-RefRecTypeA* and *cch-InterfMitigation-RefRecTypeB* to "supported", the UE shall include the parameter *cch-InterfMitigation-MaxNumCCs* to indicate that the UE supports CCH-IM on at least one arbitrary downlink CC for up to *cch-InterfMitigation-MaxNumCCs* downlink CC CA configuration. The UE shall not include the parameter *cch-InterfMitigation-MaxNumCCs* if neither *cch-InterfMitigation-RefRecTypeA* nor *cch-InterfMitigation-RefRecTypeB* is present. The UE may not perform CCH-IM on more than 1 DL CCs. For example, the UE sets "*cch-InterfMitigation-MaxNumCCs* = 3"to indicate that UE supports CCH-IM on at least one DL CC for supported non-CA, 2DL CA and 3DL CA configurations. For CA scenarios, the CCH-IM is guaranteed to be supported on at least one arbitrary component carrier. | - |
| ***cdma2000-NW-Sharing***Indicates whether the UE supports network sharing for CDMA2000. | - |
| ***ce-ClosedLoopTxAntennaSelection***Indicates whether the UE supports UL closed-loop Tx antenna selection in CE mode A, as specified in TS 36.212 [22]. | Yes |
| ***ce-CQI-AlternativeTable***Indicates whether the UE supports alternative CQI table in CE mode A. See TS 36.213 [22]. | Yes |
| ***ce-CRS-IntfMitig***Indicates whether UE supports CRS interference mitigation, i.e., value *supported* indicates UE does not rely on the CRS outside certain PRBs and subframes as defined in TS 36.133 [16], clauses 3.6.1.2 and 3.6.1.3, and TS 36.213 [23] when operating in coverage enhancement mode. | Yes |
| ***ce-CSI-RS-Feedback***Indicates whether the UE supports CSI-RS based feedback when the UE is operating in CE mode A, as specified in TS 36.213 [23]. | Yes |
| ***ce-CSI-RS-FeedbackCodebookRestriction***Indicates whether the UE supports CSI-RS based feedback with codebook subset restriction when the UE in CE is operating in CE mode A, as specified in TS 36.213 [23]. | Yes |
| ***ce-DL-ChannelQualityReporting***Indicates whether UE operating in CE mode supports aperiodic DL channel quality reporting in RRC\_CONNECTED. | Yes |
| ***ce-EUTRA-5GC***Indicates whether the UE operating in CE mode A or B supports E-UTRA/5GC. | Yes |
| ***ce-EUTRA-5GC-HO-ToNR-FDD-FR1***Indicates whether the UE operating in CE mode A or B supports handover from E-UTRA/5GC to NR FDD FR1. | Yes |
| ***ce-EUTRA-5GC-HO-ToNR-TDD-FR1***Indicates whether the UE operating in CE mode A or B supports handover from E-UTRA/5GC to NR TDD FR1. | Yes |
| ***ce-EUTRA-5GC-HO-ToNR-FDD-FR2***Indicates whether the UE operating in CE mode A or B supports handover from E-UTRA/5GC to NR FDD FR2. | Yes |
| ***ce-EUTRA-5GC-HO-ToNR-TDD-FR2***Indicates whether the UE operating in CE mode A or B supports handover from E-UTRA/5GC to NR TDD FR2-1. | Yes |
| ***ce-EUTRA-5GC-HO-ToNR-TDD-FR2-2***Indicates whether the UE operating in CE mode A or B supports handover from E-UTRA/5GC to NR TDD FR2-2. | - |
| ***ce-HARQ-AckBundling***Indicates whether the UE supports HARQ-ACK bundling in half duplex FDD in CE mode A, as specified in TS 36.212 [22] and TS 36.213 [23]. | - |
| ***ce-InactiveState***Indicates whether UE operating in CE mode supports RRC\_INACTIVE when connected to 5GC. A UE including this field also supports short eDRX cycles in RRC\_INACTIVE when connected to 5GC. | No |
| ***ce-MeasRSS-Dedicated, ce-MeasRSS-DedicatedSameRBs***Indicates whether the UE operating in CE mode A/B supports receiving neighbour cell RSS information in dedicated signalling and performing serving cell and neighbour cell measurements based on RSS in RRC\_CONNECTED as specified in TS 36.306 [5] and TS 36.133 [16]. | Yes |
| ***ce-ModeA, ce-ModeB***Indicates whether the UE supports operation in CE mode A and/or B, as specified in TS 36.211 [21] and TS 36.213 [23]. | - |
| ***crs-ChEstMPDCCH-CE-ModeA, crs-ChEstMPDCCH-CE-ModeB***Indicates whether UE operating in CE mode A/B supports using CRS for improving MPDCCH channel estimation. | Yes |
| ***crs-ChEstMPDCCH-CSI***Indicates whether UE operating in CE mode A supports CSI-based mapping for improving MPDCCH channel estimation. | Yes |
| ***crs-ChEstMPDCCH-ReciprocityTDD***Indicates whether UE operating in CE mode A supports using CRS for improving MPDCCH channel estimation with reciprocity-based candidates in TDD. | No |
| ***ceMeasurements***Indicates whether the UE supports intra-frequency RSRQ measurements and inter-frequency RSRP and RSRQ measurements in RRC\_CONNECTED, as specified in TS 36.133 [16] and TS 36.304 [4]. | - |
| ***ce-MultiTB-64QAM***Indicates whether the UE supports downlink 64QAM for multiple TB scheduling in connected mode for PDSCH when operating in CE mode A, as specified in TS 36.211 [21] and TS 36.213 [23]. This field can be included only if *ce-PUSCH-SubPRB-Allocation* is included. | Yes |
| ***ce-MultiTB-EarlyTermination***Indicates whether the UE supports early termination of PUSCH transmission for multiple TB scheduling in connected mode, as specified in TS 36.211 [21] and TS 36.213 [23].  | Yes |
| ***ce-MultiTB-FrequencyHopping***Indicates whether the UE supports frequency hopping for multiple TB scheduling for PDSCH/PUSCH in connected mode, as specified in TS 36.211 [21] and TS 36.213 [23].  | Yes |
| ***ce-MultiTB-HARQ-AckBundling***Indicates whether the UE supports downlink HARQ-ACK bundling for multiple TB scheduling in connected mode when operating in CE mode A, as specified in TS 36.211 [21] and TS 36.213 [23]. | Yes |
| ***ce-MultiTB-Interleaving***Indicates whether the UE supports TB interleaving for multiple TB scheduling in connected mode for PDSCH/PUSCH when operating in CE mode A or B, as specified in TS 36.211 [21] and TS 36.213 [23]. | Yes |
| ***ce-MultiTB-SubPRB***Indicates whether the UE supports sub-PRB allocation for multiple TB scheduling for PUSCH in connected mode, as specified in TS 36.211 [21] and TS 36.213 [23]. This field can be included only if *ce-PUSCH-SubPRB-Allocation* is included. | Yes |
| ***ce-PDSCH-14HARQProcesses, ce-PDSCH-14HARQProcesses-Alt2***Indicates whether the UE supports 14-HARQ processes, as specified in TS 36.212 [22]. | - |
| ***ce-PDSCH-64QAM***Indicates whether the UE supports 64QAM for non-repeated unicast PDSCH in CE mode A. | Yes |
| ***ce-PDSCH-FlexibleStartPRB-CE-ModeA*, *ce-PDSCH-FlexibleStartPRB-CE-ModeB*,*****ce-PUSCH-FlexibleStartPRB-CE-ModeA*, *ce-PUSCH-FlexibleStartPRB-CE-ModeB***This field indicates whether UE supports flexible starting PRB for PDSCH/PUSCH when operating in coverage enhancement mode A/B, as specified in TS 36.211 [21] and TS 36.213 [22]. | Yes |
| ***ce-PDSCH-MaxTBS***Indicates whether the UE supports downlink TBS of 1736 bits, as specified in TS 36.212 [22]. | - |
| ***ce-PDSCH-PUSCH-Enhancement***Indicates whether the UE supports new numbers of repetitions for PUSCH and modulation restrictions for PDSCH/PUSCH in CE mode A as specified in TS 36.212 [22] and TS 36.213 [23]. | No |
| ***ce-PDSCH-PUSCH-MaxBandwidth***Indicates the maximum supported PDSCH/PUSCH channel bandwidth in CE mode A and B, as specified in TS 36.212 [22] and TS 36.213 [23]. Value bw5 corresponds to 5 MHz and value bw20 corresponds to 20 MHz. If the field is absent the maximum PDSCH/PUSCH channel bandwidth in CE mode A and B is 1.4 MHz. If the setting of this parameter is 20 MHz, the max supported PUSCH channel bandwidth in CE mode A is 5 MHz. The maximum PUSCH channel bandwidth in CE mode B is 1.4 MHz regardless of the setting of this parameter. Parameter: transmission bandwidth configuration, see TS 36.101 [42], table 5.6-1. | Yes |
| ***ce-PDSCH-TenProcesses***Indicates whether the UE supports 10 DL HARQ processes in FDD in CE mode A. | Yes |
| ***ce-PUCCH-Enhancement***Indicates whether the UE supports repetition levels 64 and 128 for PUCCH in CE Mode B, as specified in TS 36.211 [21] and in TS 36.213 [23]. | No |
| ***ce-PUSCH-NB-MaxTBS***Indicates whether the UE supports 2984 bits max UL TBS in 1.4 MHz in CE mode A operation, as specified in TS 36.212 [22] and TS 36.213 [23]. | Yes |
| ***ce-PUSCH-SubPRB-Allocation***Indicates whether the UE supports sub-PRB resource allocation for PUSCH in CE mode A or B, as specified in TS 36.211 [21], TS 36.212 [22] and TS 36.213 [23]. | Yes |
| ***ce-RetuningSymbols***Indicates the number of retuning symbols in CE mode A and B as specified in TS 36.211 [21]. Value n0 corresponds to 0 retuning symbols and value n1 corresponds to 1 retuning symbol. If the field is absent the number of retuning symbols in CE mode A and B is 2. | No |
| ***ce-SchedulingEnhancement***Indicates whether the UE supports dynamic HARQ-ACK delay for HD-FDD in CE mode A as specified in TS 36.212 [22] and TS 36.213 [23]. | No |
| ***ce-SRS-Enhancement***Indicates whether the UE supports SRS coverage enhancement in TDD with support of SRS combs 2 and 4 as specified in TS 36.213 [23]. This field can be included only if *ce-SRS-EnhancementWithoutComb4* is not included. | Yes |
| ***ce-SRS-EnhancementWithoutComb4***Indicates whether the UE supports SRS coverage enhancement in TDD with support of SRS comb 2 but without support of SRS comb 4 as specified in TS 36.213 [23]. This field can be included only if *ce-SRS-Enhancement* is not included. | - |
| ***ce-SwitchWithoutHO***Indicates whether the UE supports switching between normal mode and enhanced coverage mode without handover. | - |
| ***ce-UL-HARQ-ACK-Feedback***This field indicates whether UE supports uplink HARQ ACK feedback when operating in coverage enhancement, as specified in TS36.213 [22]. | Yes |
| ***channelMeasRestriction***Indicates for a particular transmission mode whether the UE supports channel measurement restriction. | Yes |
| ***cho***Indicates whether the UE supports conditional handover including execution condition, candidate cell configuration and maximum 8 candidate cells. | Yes |
| ***cho-Failure***Indicates whether the UE supports conditional handover during re-establishment procedure when the selected cell is configured as candidate cell for condition handover. | Yes |
| ***cho-FDD-TDD***Indicates whether the UE supports conditional handover between FDD and TDD cells. | No |
| ***cho-TwoTriggerEvents***Indicates whether the UE supports 2 trigger events for same execution condition. It is mandatory supported if the UE suppors *cho*. | Yes |
| ***codebook-HARQ-ACK***Indicates whether the UE supports determining HARQ ACK codebook size based on the DAI-ased solution and/or the number of configured CCs. The first bit is set to "1" if the UE supports the DAI-based codebook size determination. The second bit is set to "1" if the UE supports the codebook determination based on the number of configured CCs. | No |
| ***commMultipleTx***Indicates whether the UE supports multiple transmissions of sidelink communication to different destinations in one SC period. If *commMultipleTx-r13* is set to supported then the UE support 8 transmitting sidelink processes. | - |
| ***commSimultaneousTx***Indicates whether the UE supports simultaneous transmission of EUTRA and sidelink communication (on different carriers) in all bands for which the UE indicated sidelink support in a band combination (using *commSupportedBandsPerBC*). | - |
| ***commSupportedBands***Indicates the bands on which the UE supports sidelink communication, by an independent list of bands i.e. separate from the list of supported E-UTRA band, as indicated in *supportedBandListEUTRA*. | - |
| ***commSupportedBandsPerBC***Indicates, for a particular band combination, the bands on which the UE supports simultaneous reception of EUTRA and sidelink communication. If the UE indicates support simultaneous transmission (using *commSimultaneousTx*), it also indicates, for a particular band combination, the bands on which the UE supports simultaneous transmission of EUTRA and sidelink communication. The first bit refers to the first band included in *commSupportedBands*, with value 1 indicating sidelink is supported. | - |
| ***configN (in MIMO-CA-ParametersPerBoBCPerTM)***If signalled, the field indicates for a particular transmission mode whether the UE supports non-precoded EBF/ FD-MIMO (class A) related configuration N for the concerned band combination. | - |
| ***configN (in MIMO-UE-ParametersPerTM)***Indicates for a particular transmission mode whether the UE supports non-precoded EBF/ FD-MIMO (class A) related configuration N for band combinations for which the concerned capabilities are not signalled. | Yes |
| ***continueEHC-Context***Indicates that the UE supports EHC context continuation operation where the UE keeps the established EHC context(s) upon PDCP re-establishment, as specified in TS 36.323 [8]. | No |
| ***crossCarrierScheduling*** | Yes |
| ***crossCarrierScheduling-B5C***Indicates whether the UE supports cross carrier scheduling beyond 5 DL CCs. | No |
| ***crossCarrierSchedulingLAA-DL***Indicates whether the UE supports cross-carrier scheduling from a licensed carrier for LAA cell(s) for downlink. This field can be included only if *downlinkLAA* is included. | - |
| ***crossCarrierSchedulingLAA-UL***Indicates whether the UE supports cross-carrier scheduling from a licensed carrier for LAA cell(s) for uplink. This field can be included only if *uplinkLAA* is included. | - |
| ***crs-DiscoverySignalsMeas***Indicates whether the UE supports CRS based discovery signals measurement, and PDSCH/EPDCCH RE mapping with zero power CSI-RS configured for discovery signals. | Yes |
| ***crs-IM-TM1-toTM9-OneRX-Port***Indicates whether the DL Cateogry 1bis UE ot the DL Category M2 UE supports CRS interference mitigation (IM) while operating in the following transmission modes (TM): TM 1, TM 2, …, TM 8 and TM 9.  | No |
| ***crs-InterfHandl***Indicates whether the UE supports CRS interference handling. | Yes |
| ***crs-InterfMitigationTM10***The field defines whether the UE supports CRS interference mitigation in transmission mode 10. The UE supporting the *crs-InterfMitigationTM10* capability shall also support the *crs-InterfHandl* capability. | No |
| ***crs-InterfMitigationTM1toTM9***Indicates whether the UE supports CRS interference mitigation (IM) while operating in the following transmission modes (TM): TM 1, TM 2, …, TM 8 and TM 9. The UE shall not include the field if it does not support CRS IM in TMs 1-9. If the field is present, the UE supports CRS-IM on at least one arbitrary downlink CC for up to *crs-InterfMitigationTM1toTM9-r13* downlink CC CA configuration. The UE signals *crs-InterfMitigationTM1toTM9-r13* value to indicate the maximum *crs-InterfMitigationTM1toTM9-r13* downlink CC CA configuration where UE may apply CRS IM. For example, the UE sets "*crs-InterfMitigationTM1toTM9-r13* = 3" to indicate that the UE supports CRS-IM on at least one DL CC for supported non-CA, 2DL CA and 3DL CA configurations. The UE supporting the *crs-InterfMitigationTM1toTM9-r13* capability shall also support the *crs-InterfHandl-r11* capability. | - |
| ***crs-IntfMitig***Indicate whether the UE supports CRS interference mitigation as specified in TS 36.133 [16], clause 3.6.1.1. | Yes |
| ***crs-LessDwPTS***Indicates whether the UE supports TDD special subframe configuration 10 without CRS transmission on the 5th symbol of DwPTS, i.e. *ssp10-CRS-LessDwPTS*, as specified in TS 36.211 [17]*.*  | - |
| ***csi-ReportingAdvanced, csi-ReportingAdvancedMaxPorts (in MIMO-CA-ParametersPerBoBCPerTM)***If signalled, the field indicates that for a particular transmission mode, the maximum number of CSI-RS ports supported by the UE for advanced CSI reporting is different in the concerned band of band combination than the value indicated by the field *csi-ReportingAdvanced* or *csi-ReportingAdvancedMaxPorts* in *MIMO-UE-ParametersPerTM*. The UE shall not include both *csi-ReportingAdvanced* and *csi-ReportingAdvancedMaxPorts* for a particular transmission mode in the concerned band of band combination. | - |
| ***csi-ReportingAdvanced (in MIMO-UE-ParametersPerTM)***Indicates for a particular transmission mode the maximum number of CSI-RS ports supported by the UE for advanced CSI reporting. The field *csi-ReportingAdvanced* indicates 32 CSI-RS ports. The UE shall not include both *csi-ReportingAdvanced* and *csi-ReportingAdvancedMaxPorts* for a particular transmission mode.  | Yes |
| ***csi-ReportingAdvancedMaxPorts (in MIMO-UE-ParametersPerTM)***Indicates for a particular transmission mode the maximum number of CSI-RS ports supported by the UE for advanced CSI reporting. The field *csi-ReportingAdvancedMaxPorts* indicates 8, 12, 16, 20, 24 or 28 CSI-RS ports. The UE shall not include both *csi-ReportingAdvanced* and *csi-ReportingAdvancedMaxPorts* for a particular transmission mode. | - |
| ***csi-ReportingNP (in MIMO-CA-ParametersPerBoBCPerTM)***If signalled, value *different* indicates that for a particular transmission mode, the CSI reporting on non-precoded CSI-RS with 20, 24, 28 or 32 antenna ports for the concerned band of band combination is different than the value indicated by field *csi-ReportingNP* in *MIMO-UE-ParametersPerTM*. | - |
| ***csi-ReportingNP (in MIMO-UE-ParametersPerTM)***Indicates for a particular transmission mode whether the UE supports CSI reporting on non-precoded CSI-RS with 20, 24, 28, or 32 antenna ports for band combinations for which the concerned capabilities are not signalled in *MIMO-CA-ParametersPerBoBCPerTM*, and the FD-MIMO processing capability condition as described in NOTE 8 is satisfied. | Yes |
| ***csi-RS-DiscoverySignalsMeas***Indicates whether the UE supports CSI-RS based discovery signals measurement. If this field is included, the UE shall also include *crs-DiscoverySignalsMeas*. | Yes |
| ***csi-RS-DRS-RRM-MeasurementsLAA***Indicates whether the UE supports performing RRM measurements on LAA cell(s) based on CSI-RS-based DRS. This field can be included only if *downlinkLAA* is included. | - |
| ***csi-RS-EnhancementsTDD***Indicates for a particular transmission mode whether the UE supports CSI-RS enhancements applicable for TDD. | Yes |
| ***csi-SubframeSet***Indicates whether the UE supports REL-12 DL CSI subframe set configuration, REL-12 DL CSI subframe set dependent CSI measurement/feedback, configuration of up to 2 CSI-IM resources for a CSI process with no more than 4 CSI-IM resources for all CSI processes of one frequency if the UE supports tm10, configuration of two ZP-CSI-RS for tm1 to tm9, PDSCH RE mapping with two ZP-CSI-RS configurations, and EPDCCH RE mapping with two ZP-CSI-RS configurations if the UE supports EPDCCH. This field is only applicable for UEs supporting TDD.  | Yes |
| ***csi-SubframeSet2ForDormantSCell***Indicates whether the UE supports second CSI subframe set for periodic CSI reporting for dormant serving cells. A UE that indicates support of this field shall also indicate support for *dormantSCellState-r15*. This field is only applicable for UEs supporting TDD. | - |
| ***dataInactMon***Indicates whether the UE supports the data inactivity monitoring as specified in TS 36.321 [6]. | - |
| ***dc-Support***Including this field indicates that the UE supports synchronous DC and power control mode 1. Including this field for a band combination entry comprising of single band entry indicates that the UE supports intra-band contiguous DC. Including this field for a band combination entry comprising of two or more band entries, indicates that the UE supports DC for these bands and that the serving cells corresponding to a band entry shall belong to one cell group (i.e. MCG or SCG). Including field *asynchronous* indicates that the UE supports asynchronous DC and power control mode 2. Including this field for a TDD/FDD band combination indicates that the UE supports TDD/FDD DC for this band combination. | - |
| ***delayBudgetReporting***Indicates whether the UE supports delay budget reporting. | No |
| ***demodulationEnhancements***This field defines whether the UE supports advanced receiver in SFN scenario (350 km/h) as specified in TS 36.101 [42]. | - |
| ***demodulationEnhancements2***This field defines whether the UE supports further enhanced receiver in HST-SFN scenario (up to 500 km/h velocity) as specified in TS 36.101 [42]. | - |
| ***densityReductionNP, densityReductionBF***Indicates whether the UE supports CSI-RS density reduction with values 1, 1/2 and 1/3 for non-precoded CSI-RS and beamformed CSI-RS respectively. | Yes |
| ***deviceType***UE may set the value to "*noBenFromBatConsumpOpt*" when it does not foresee to particularly benefit from NW-based battery consumption optimisation. Absence of this value means that the device does benefit from NW-based battery consumption optimisation. | - |
| ***diffFallbackCombReport***Indicates that the UE supports reporting of UE radio access capabilities for the CA band combinations asked by the eNB as well as, if any, reporting of different UE radio access capabilities for their fallback band combination as specified in TS 36.306 [5]. The UE does not report fallback combinations if their UE radio access capabilities are the same as the ones for the CA band combination asked by the eNB. | - |
| ***differentFallbackSupported***Indicates that the UE supports different capabilities for at least one fallback case of this band combination. | - |
| ***directMCG-SCellActivationResume***Indicates whether the UE supports having an E-UTRA MCG SCell configured in activated SCell state. | - |
| ***directSCellActivation***Indicates whether the UE supports having an E-UTRA SCell configured in activated SCell state in the *RRCConnectionReconfiguration* message. This field is applicable to both LTE standalone and LTE-DC. | - |
| ***directSCellHibernation***Indicates whether the UE supports having an SCell configured in dormant SCell state. | - |
| ***directSCG-SCellActivationNEDC***Indicates whether the UE supports having an E-UTRA SCG SCell configured in activated SCell state in the *RRCConnectionReconfiguration* message contained in the NR *RRCReconfiguration* message, as defined in TS 36.321 [6] and TS 38.331 [82].If the UE indicates support of *directSCG-SCellActivationNEDC-r16*, the UE shall also indicate support of *ne-dc* as specified in TS 38.331 [82]. | - |
| ***directSCG-SCellActivationResume***Indicates whether the UE supports having an E-UTRA SCG SCell configured in activated SCell state. | - |
| ***discInterFreqTx***Indicates whether the UE support sidelink discovery announcements either a) on the primary frequency only or b) on other frequencies also, regardless of the UE configuration (e.g. CA, DC). The UE may set discInterFreqTx to supported when having a separate transmitter or if it can request sidelink discovery transmission gaps. | - |
| ***discoverySignalsInDeactSCell***Indicates whether the UE supports the behaviour on DL signals and physical channels when SCell is deactivated and discovery signals measurement is configured as specified in TS 36.211 [21], clause 6.11A. This field is included only if UE supports carrier aggregation and includes *crs-DiscoverySignalsMeas*. | Yes |
| ***discPeriodicSLSS***Indicates whether the UE supports periodic (i.e. not just one time before sidelink discovery announcement) Sidelink Synchronization Signal (SLSS) transmission and reception for sidelink discovery. | - |
| ***discScheduledResourceAlloc***Indicates whether the UE supports transmission of discovery announcements based on network scheduled resource allocation. | - |
| ***disc-UE-SelectedResourceAlloc***Indicates whether the UE supports transmission of discovery announcements based on UE autonomous resource selection. | - |
| ***disc***-***SLSS***Indicates whether the UE supports Sidelink Synchronization Signal (SLSS) transmission and reception for sidelink discovery. | - |
| ***discSupportedBands***Indicates the bands on which the UE supports sidelink discovery. One entry corresponding to each supported E-UTRA band, listed in the same order as in *supportedBandListEUTRA*. | - |
| ***discSupportedProc***Indicates the number of processes supported by the UE for sidelink discovery. | - |
| ***discSysInfoReporting***Indicates whether the UE supports reporting of system information for inter-frequency/PLMN sidelink discovery. | - |
| ***dl-256QAM***Indicates whether the UE supports 256QAM in DL on the band. | - |
| ***dl-1024QAM***Indicates whether the UE supports 1024QAM in DL on the band or on the band within the band combination. When *dl-1024QAM-ScalingFactor* and *dl-1024QAM-TotalWeightedLayers* are included, the UE supports 1024QAM in a set of CCs in a band combination if the CCs belong to bands indicated to support 1024QAM in that band combination and the 1024QAM processing capability condition as specified in equation 4.3.5.31-1 in TS 36.306 [5] is satisfied. | - |
| ***dl-1024QAM-ScalingFactor***Indicates scaling factor for processing a CC configured with 1024QAM with respect to a CC not configured with 1024QAM as described in 4.3.5.31 in TS 36.306 [5]. Value *v1* indicates 1, value *v1dot2* indicates 1.2 and value *v1dot25* indicates 1.25. | - |
| ***dl-1024QAM-TotalWeightedLayers***Indicates total number of weighted layers the UE can process for 1024QAM as described in 4.3.5.31 in TS 36.306 [5]. Actual value = (10 + indicated value x 2), i.e., value 0 indicates 10 layers, value 1 indicates 12 layers and so on. | - |
| ***dl-1024QAM-Slot***Indicates whether the UE supports 1024QAM in DL on the band for slot TTI operation. | - |
| ***dl-1024QAM-SubslotTA-1***Indicates whether the UE supports 1024QAM in DL on the band for subslot TTI operation with TA set 1. | - |
| ***dl-1024QAM-SubslotTA-2***Indicates whether the UE supports 1024QAM in DL on the band for subslot TTI operation with TA set 2, dmrsBasedSPDCCH-nonMBSFN | - |
| ***dl-DedicatedMessageSegmentation***Indicates whether the UE supports reception of segmented DL RRC messages. | - |
| ***dmrs-BasedSPDCCH-MBSFN***Indicates whether the UE supports sDCI monitoring in DMRS based SPDCCH for MBSFN subframe. If UE supports this, it also provides the corresponding DMRS based SPDCCH capability in *min-Proc-TimelineSubslot.* | Yes |
| ***dmrs-BasedSPDCCH-nonMBSFN***Indicates whether the UE supports sDCI monitoring in DMRS based SPDCCH for non-MBSFN subframe. If UE supports this, it also provides the corresponding DMRS based SPDCCH capability in *min-Proc-TimelineSubslot.* | Yes |
| ***dmrs-Enhancements (in MIMO-CA-ParametersPerBoBCPerTM)***If signalled, the field indicates for a particular transmission mode, that for the concerned band combination the DMRS enhancements are different than the value indicated by field *dmrs-Enhancements* in *MIMO-UE-ParametersPerTM*. | - |
| ***dmrs-Enhancements (in MIMO-UE-ParametersPerTM)***Indicates for a particular transmission mode whether the UE supports DMRS enhancements for the indicated transmission mode. | Yes |
| ***dmrs-LessUpPTS***Indicates whether the UE supports not to transmit DMRS for PUSCH in UpPTS. | No |
| ***dmrs-OverheadReduction***Indicates whether the UE supports OCC4 for rank 3 and 4 transmission as specified in clause 5.3.3.1.5C of TS 36.212 [22]. | Yes |
| ***dmrs-PositionPattern***Indicates whether the UE supports uplink DMRS position pattern 'D D D' in subslot #5 with application of the 1/6 as the TBS scaling factor. | Yes |
| ***dmrs-RepetitionSubslotPDSCH***Indicates whether the UE supports back-to-back 3/4-layer DMRS reception in two consecutive subslots across subframe boundary for subslot-PDSCH. | Yes |
| ***dmrs-SharingSubslotPDSCH***Indicates whether the UE supports DMRS sharing in two consecutive subslots across subframe boundary for subslot-PDSCH. | Yes |
| ***dormantSCellState***Indicates whether UE supports Dormant SCell state (i.e. SCell state with CQI and RRM measurement reporting but no PDCCH monitoring). | - |
| ***downlinkLAA***Presence of the field indicates that the UE supports downlink LAA operation including identification of downlink transmissions on LAA cell(s) for full downlink subframes, decoding of common downlink control signalling on LAA cell(s), CSI feedback for LAA cell(s), RRM measurements on LAA cell(s) based on CRS-based DRS. | - |
| ***drb-TypeSCG***Indicates whether the UE supports SCG bearer. | - |
| ***drb-TypeSplit***Indicates whether the UE supports split bearer except for PDCP data transfer in UL.  | - |
| ***dtm***Indicates whether the UE supports DTM in GERAN. | - |
| ***dummy***This field is not used in the specification. It shall not be sent by the UE. | - |
| ***earlyData-UP***Indicates whether the UE supports UP-EDT when connected to EPC. | - |
| ***earlyData-UP-5GC***Indicates whether the UE supports UP-EDT when connected to 5GC. | - |
| ***earlySecurityReactivation***Indicates whether the UE supports early security reactivation when resuming a suspended RRC connection. | - |
| ***e-CSFB-1XRTT***Indicates whether the UE supports enhanced CS fallback to CDMA2000 1xRTT or not. | Yes |
| ***e-CSFB-ConcPS-Mob1XRTT***Indicates whether the UE supports concurrent enhanced CS fallback to CDMA2000 1xRTT and PS handover/ redirection to CDMA2000 HRPD. | Yes |
| ***e-CSFB-dual-1XRTT***Indicates whether the UE supports enhanced CS fallback to CDMA2000 1xRTT for dual Rx/Tx configuration. This bit can only be set to supported if *tx-Config1XRTT* and *rx-Config1XRTT* are both set to dual. | Yes |
| ***e-HARQ-Pattern-FDD***Indicates whether the UE supports enhanced HARQ pattern for TTI bundling operation for FDD. | Yes |
| ***ehc***Indicates that the UE supports Ethernet header compression and decompression using EHC protocol, as specified in TS 36.323 [8] and in Annex A of TS 38.323 [83]. The UE indicating this capability and indicating support for at least one ROHC profile, shall support simultaneous configuration of EHC and ROHC on different DRBs. | No |
| ***eLCID-Support***Indicates whether the UE supports LCID "10000" and MAC PDU subheader containing the eLCID field as described in TS 36.321 [6]. | - |
| ***emptyUnicastRegion***Indicates whether the UE supports unicast reception in subframes with empty unicast control region as described in TS 36.213 [23] clause 12. This field can be included only if *unicast-fembmsMixedSCell* and *crossCarrierScheduling* are included. | No |
| ***en-DC***Indicates whether the UE supports EN-DC. | - |
| ***endingDwPTS***Indicates whether the UE supports reception ending with a subframe occupied for a DwPTS-duration as described in TS 36.211 [21] and TS 36.213 [23]. This field can be included only if *downlinkLAA* is included. | - |
| ***Enhanced-4TxCodebook***Indicates whether the UE supports enhanced 4Tx codebook*.* | No |
| ***enhancedDualLayerTDD***Indicates whether the UE supports enhanced dual layer (PDSCH transmission mode 8) for TDD or not. | - |
| ***ePDCCH***Indicates whether the UE can receive DCI on UE specific search space on Enhanced PDCCH. | Yes |
| ***epdcch-SPT-differentCells***Indicates whether the UE supports EPDCCH and short processing time on different serving cells. | Yes |
| ***epdcch-STTI-differentCells***Indicates whether the UE supports EPDCCH and sTTI on different serving cells. | Yes |
| ***e-RedirectionUTRA*** | Yes |
| ***e-RedirectionUTRA-TDD***Indicates whether the UE supports enhanced redirection to UTRA TDD to multiple carrier frequencies both with and without using related SIB provided by *RRCConnectionRelease* or not. | Yes |
| ***etws-CMAS-RxInConnCE-ModeA, etws-CMAS-RxInConn***Indicates whether the UE operating in CE mode A/B supports reception of ETWS/CMAS indication in RRC\_CONNECTED mode as specified in TS 36.212 [22]. | - |
| ***eutra-5GC***Indicates whether the UE supports E-UTRA/5GC.  | Yes |
| ***eutra-5GC-HO-ToNR-FDD-FR1***Indicates whether the UE supports handover from E-UTRA/5GC to NR FDD FR1.  | Yes |
| ***eutra-5GC-HO-ToNR-TDD-FR1***Indicates whether the UE supports handover from E-UTRA/5GC to NR TDD FR1.  | Yes |
| ***eutra-5GC-HO-ToNR-FDD-FR2***Indicates whether the UE supports handover from E-UTRA/5GC to NR FDD FR2.  | Yes |
| ***eutra-5GC-HO-ToNR-TDD-FR2***Indicates whether the UE supports handover from E-UTRA/5GC to NR TDD FR2-1. | Yes |
| ***eutra-5GC-HO-ToNR-TDD-FR2-2***Indicates whether the UE supports handover from E-UTRA/5GC to NR TDD FR2-2. | - |
| ***eutra-CGI-Reporting-ENDC***Indicates whether the UE supports Intra-RAT report CGI procedure when it is configured with (NG) EN-DC wherein either MN and SN have different DRX cycles, or on-duration configured by MN does not contain on-duration configured by SN if their DRX cycles are same. | Yes |
| ***eutra-CGI-Reporting-NEDC***Indicates whether the UE supports acquisition of relevant information from a neighbouring E-UTRA cell by reading the SI of the neighbouring cell and reporting the acquired information to the network when the NE-DC is configured. | Yes |
| ***eutra-EPC-HO-ToNR-FDD-FR1***Indicates whether the UE supports handover from E-UTRA/EPC to NR FDD FR1.  | Yes |
| ***eutra-EPC-HO-ToNR-TDD-FR1***Indicates whether the UE supports handover from E-UTRA/EPC to NR TDD FR1.  | Yes |
| ***eutra-EPC-HO-ToNR-FDD-FR2***Indicates whether the UE supports handover from E-UTRA/EPC to NR FDD FR2.  | Yes |
| ***eutra-EPC-HO-ToNR-TDD-FR2***Indicates whether the UE supports handover from E-UTRA/EPC to NR TDD FR2-1. | Yes |
| ***eutra-EPC-HO-ToNR-TDD-FR2-2***Indicates whether the UE supports handover from E-UTRA/EPC to NR TDD FR2-2. | - |
| ***eutra-EPC-HO-EUTRA-5GC***Indicates whether the UE supports handover between E-UTRA/EPC and E-UTRA/5GC.  | Yes |
| ***eutra-IdleInactiveMeasurements***Indicates whether UE supports reporting measurements performed during RRC\_IDLE or RRC\_INACTIVE. | No |
| ***eutra-SI-AcquisitionForHO-ENDC***Indicates whether the UE supports, upon configuration of *si-RequestForHO* by the network, acquisition of relevant information from a neighbouring E-UTRA cell by reading the SI of the neighbouring cell using autonomous gaps and reporting the acquired information to the network. | Yes |
| ***eventB2***Indicates whether the UE supports event B2. A UE supporting NR SA operation shall set this bit to *supported*. | - |
| ***eventD1-MeasReportTrigger***This field indicates whether the UE supports location-based measurement report triggering in RRC\_CONNECTED in earth fixed cell (i.e. event D1). | - |
| ***eventD2-MeasReportTrigger***This field indicates whether the UE supports location-based measurement report triggering in RRC\_CONNECTED in earth moving cell (i.e. event D2). | - |
| ***extendedBand-n77***This field is only applicable for UEs that indicate support for band n77. If present, the UE supports the restriction to 3450 - 3550 MHz and 3700 - 3980 MHz ranges of band n77 in the USA as specified in Note 12 of Table 5.2-1 in TS 38.101-1 [85]. If absent, the UE supports only restriction to the 3700 - 3980 MHz range of band n77 in the USA. A UE that indicates this field shall support NS value 55 as specified in TS 38.101-1 [85]. | - |
| ***extendedBand-n77-2***This field is only applicable for UEs that indicate support for band n77. If present, the UE supports the restriction to 3450 - 3650 MHz and 3650 - 3980 ranges of band n77 in Canada as specified in Note 12 of Table 5.2-1 in TS 38.101-1 [85]. If absent, the UE supports only restriction to the 3450 - 3650 MHz range of band n77 in Canada. A UE that indicates this field shall also support NS value 57 as specified in TS 38.101-1 [85]. | - |
| ***extendedFreqPriorities***Indicates whether the UE supports extended E-UTRA frequency priorities indicated by *cellReselectionSubPriority* field. A UE supporting NR SA operation shall set this bit to *supported*. | - |
| ***extendedLCID-Duplication***Indicates whether the UE supports use of extended LCIDs 32-38 for PDCP duplication. | - |
| ***extendedLongDRX***Indicates whether the UE supports extended long DRX cycle values of 5.12s and 10.24s in RRC\_CONNECTED. | - |
| ***extendedMAC-LengthField***Indicates whether the UE supports the MAC header with L field of size 16 bits as specified in TS 36.321 [6], clause 6.2.1. | - |
| ***extendedMaxMeasId***Indicates whether the UE supports extended number of measurement identies as defined by *maxMeasId-r12*. | No |
| ***extendedMaxObjectId***Indicates whether the UE supports extended number of measurement object identies as defined by *maxObjectId-r13*. | No |
| ***extendedNumberOfDRBs***Indicates whether the UE supports up to 15 DRBs. The UE shall support any combination of RLC AM and RLC UM entities for the configured DRBs. | - |
| ***extendedPollByte***Indicates whether the UE supports extended pollByte values as defined by *pollByte-r14*. | - |
| ***extended-RLC-LI-Field***Indicates whether the UE supports 15 bit RLC length indicator. | - |
| ***extendedRLC-SN-SO-Field***Indicates whether the UE supports 16 bits of RLC sequence number and segmentation offset. | - |
| ***extendedRSRQ-LowerRange***Indicates whether the UE supports the extended RSRQ lower value range from -34dB to -19.5dB in measurement configuration and reporting as specified in TS 36.133 [16]. | No |
| ***fdd-HARQ-TimingTDD***Indicates whether UE supports FDD HARQ timing for TDD SCell when configured with TDD PCell. | Yes |
| ***featureGroupIndicators, featureGroupIndRel9Add, featureGroupIndRel10***The definitions of the bits in the bit string are described in Annex B.1 (for *featureGroupIndicators* and *featureGroupIndRel9Add*) and in Annex C.1 (for *featureGroupIndRel10*). | Yes |
| ***featureSetsDL-PerCC***In MR-DC, indicates a set of features that the UE supports on one component carrier in a bandwidth class for a band in a given band combination. The UE shall hence include at least as many *FeatureSetDL-PerCC-Id* in this list as the number of carriers it supports according to the *ca-bandwidthClassDL*, except if indicating additional functionality by reducing the number of *FeatureSetDownlinkPerCC-Id* in the feature set. The order of the elements in this list is not relevant, i.e., the network may configure any of the carriers in accordance with any of the *FeatureSetDL-PerCC-Id* in this list. | - |
| ***FeatureSetDL-PerCC-Id***In MR-DC, indicates the index position of the *FeatureSetDL-PerCC-r15* in the *featureSetsDL-PerCC-r15* list. Value 0 corresponds to the first element in the list, value 1 corresponds to the second element in the list, and so on. Value 32 is not used. | - |
| ***featureSetsUL-PerCC***In MR-DC, indicates a set of features that the UE supports on one component carrier in a bandwidth class for a band in a given band combination. The UE shall hence include at least as many *FeatureSetUL-PerCC-Id* in this list as the number of carriers it supports according to the *ca-bandwidthClassUL*, except if indicating additional functionality by reducing the number of *FeatureSetDownlinkPerCC-Id* in the feature set. The order of the elements in this list is not relevant, i.e., the network may configure any of the carriers in accordance with any of the *FeatureSetUL-PerCC-Id* in this list. | - |
| ***FeatureSetUL-PerCC-Id***In MR-DC, indicates the index position of the *FeatureSetUL-PerCC-r15* in the *featureSetsUL-PerCC-r15* list. Value 0 corresponds to the first element in the list, value 1 corresponds to the second element in the list, and so on. Value 32 is not used. | - |
| ***fembmsMixedCell***Indicates whether the UE in RRC\_CONNECTED supports MBMS reception with 15 kHz subcarrier spacings via MBSFN from FeMBMS/Unicast mixed cells on a frequency indicated in an *MBMSInterestIndication* message. |  |
| ***fembmsDedicatedCell***Indicates whether the UE in RRC\_CONNECTED supports MBMS reception with 15 kHz subcarrier spacings via MBSFN from MBMS-dedicated cells on a frequency indicated in an *MBMSInterestIndication* message. |  |
| ***flexibleUM-AM-Combinations***Indicates whether the UE supports any combination of RLC UM and RLC AM bearers as long as the total number of bearers is at most 8, regardless of what FGI20 indicates. | - |
| ***flightPathPlan***Indicates whether UE supports reporting of flight path plan information. | - |
| ***fourLayerTM3-TM4***Indicates whether the UE supports 4-layer spatial multiplexing for TM3 and TM4. | - |
| ***fourLayerTM3-TM4 (in FeatureSetDL-PerCC)***Indicates whether the UE supports 4-layer spatial multiplexing for TM3 and TM4 for MR-DC within the indicated feature set. If this field is absent, UE supports two layer MIMO for TM3/TM4. | - |
| ***fourLayerTM3-TM4-perCC***Indicates whether the UE supports 4-layer spatial multiplexing for TM3 and TM4 for the component carrier. | - |
| ***frameStructureType-SPT***This field indicates the supported FS-type(s) for short processing time. The UE capability is reported per band combination. The reported FS-type(s) apply to the reported *maxNumberCCs-SPT-r15* for the given band combination. | - |
| ***freqBandPriorityAdjustment***Indicates whether the UE supports the prioritization of frequency bands in *multiBandInfoList* over the band in *freqBandIndicator* as defined by *freqBandIndicatorPriority-r12*. | - |
| ***freqBandRetrieval***Indicates whether the UE supports reception of *requestedFrequencyBands.* | - |
| ***gaplessMeas-FR2-maxCC***Indicates whether the UE supports inter-RAT NR FR2 measurement without measurement gap as specified in clause 9.1.2 of TS 38.133 [84] while the number of configured serving cells is less than or equal to the indicated number. This field is applicable when only E-UTRA serving cells are configured. The UE reporting this field and supporting (NG)EN-DC shall not indicate support of *independentGapConfig* in *MeasAndMobParametersMRDC* (defined in TS 38.306 [87]). | - |
| ***gNB-ID-Length-Reporting-NR-EN-DC***Indicates whether the UE supports Inter-RAT gNB ID length reporting towards NR cell when it is configured with (NG)EN-DC. If the UE supports *reportCGI-NR-EN-DC-r15*, the UE shall support the *gNB-ID-Length-Reporting-NR-EN-DC-r17*. | - |
| ***gNB-ID-Length-Reporting-NR-NoEN-DC***Indicates whether the UE supports Inter-RAT gNB ID length reporting towards cell when it is not configured with (NG)EN-DC. If the UE supports *reportCGI-NR-NoEN-DC-r15*, the UE shall support *gNB-ID-Length-Reporting-NR-NoEN-DC-r17*. | - |
| ***halfDuplex***If *halfDuplex* is set to true, only half duplex operation is supported for the band, otherwise full duplex operation is supported. | - |
| ***heightMeas***Indicates whether UE supports the measurement events H1/H2. | - |
| ***ho-EUTRA-5GC-FDD-TDD***Indicates whether the UE supports handover between E-UTRA/5GC FDD and E-UTRA/5GC TDD.  | No |
| ***ho-InterfreqEUTRA-5GC***Indicates whether the UE supports inter frequency handover within E-UTRA/5GC.  | Yes |
| ***hybridCSI***Indicates whether the UE supports hybrid CSI transmission as described in TS 36.213 [23]. | Yes |
| ***idleInactiveValidityAreaList***Indicates whether the UE supports list of validity areas for measurements during RRC\_IDLE and RRC\_INACTIVE. | No |
| ***immMeasBT***Indicates whether the UE supports Bluetooth measurements in RRC connected mode. | - |
| ***immMeasUnComBarPre***Indicates whether the UE supports uncompensated barometric pressure measurements in RRC connected mode. | - |
| ***immMeasWLAN***Indicates whether the UE supports WLAN measurements in RRC connected mode. | - |
| ***ims-VoiceOverMCG-BearerEUTRA-5GC***Indicates whether the UE supports IMS voice over NR PDCP for MCG bearer for E-UTRA/5GC. | No |
| ***ims-VoiceOverNR-FR1***Indicates whether the UE supports IMS voice over NR FR1. | No |
| ***ims-VoiceOverNR-FR2***Indicates whether the UE supports IMS voice over NR FR2-1. | No |
| ***ims-VoiceOverNR-FR2-2***Indicates whether the UE supports IMS voice over NR FR2-2. | - |
| ***ims-VoiceOverNR-PDCP-MCG-Bearer***Indicates whether the UE supports IMS voice over NR PDCP with only MCG RLC bearer. | Yes |
| ***ims-VoiceOverNR-PDCP-SCG-Bearer***Indicates whether the UE supports IMS voice over NR PDCP with only SCG RLC bearer when configured with EN-DC. | Yes |
| ***ims-VoNR-PDCP-SCG-NGENDC***Indicates whether the UE supports IMS voice over NR PDCP with only SCG RLC bearer when configured with NGEN-DC. | Yes |
| ***inactiveState***Indicates whether the UE supports RRC\_INACTIVE. | No |
| ***incMonEUTRA***Indicates whether the UE supports increased number of E-UTRA carrier monitoring in RRC\_IDLE and RRC\_CONNECTED, as specified in TS 36.133 [16]. | No |
| ***incMonUTRA***Indicates whether the UE supports increased number of UTRA carrier monitoring in RRC\_IDLE and RRC\_CONNECTED, as specified in TS 36.133 [16]. | No |
| ***inDeviceCoexInd***Indicates whether the UE supports in-device coexistence indication as well as autonomous denial functionality. | Yes |
| ***inDeviceCoexInd-ENDC***Indicates whether the UE supports in-device coexistence indication for (NG)EN-DC operation. This field can be included only if *inDeviceCoexInd* is included. The UE supports *inDeviceCoexInd-ENDC* in the same duplexing modes as it supports *inDeviceCoexInd*. | - |
| ***inDeviceCoexInd-HardwareSharingInd***Indicates whether the UE supports indicating hardware sharing problems when sending the *InDeviceCoexIndication*, as well as omitting the TDM assistance information. A UE that supports hardware sharing indication shall also indicate support of LAA operation. | - |
| ***inDeviceCoexInd-UL-CA***Indicates whether the UE supports UL CA related in-device coexistence indication. This field can be included only if *inDeviceCoexInd* is included. The UE supports *inDeviceCoexInd-UL-CA* in the same duplexing modes as it supports *inDeviceCoexInd*. | - |
| ***interBandTDD-CA-WithDifferentConfig***Indicates whether the UE supports inter-band TDD carrier aggregation with different UL/DL configuration combinations. The first bit indicates UE supports the configuration combination of SCell DL subframes are a subset of PCell and PSCell by SIB1 configuration and the configuration combination of SCell DL subframes are a superset of PCell and PSCell by SIB1 configuration; the second bit indicates UE supports the configuration combination of SCell DL subframes are neither superset nor subset of PCell and PSCell by SIB1 configuration. This field is included only if UE supports inter-band TDD carrier aggregation. | - |
| ***interBandPowerSharingAsyncDAPS***Indicates whether the UE supports power sharing for asynchronous inter-band DAPS handovers. | - |
| ***interBandPowerSharingSyncDAPS***Indicates whether the UE supports power sharing for synchronous inter-band DAPS handovers. | - |
| ***interferenceMeasRestriction***Indicates whether the UE supports interference measurement restriction. | Yes |
| ***interFreqAsyncDAPS***Indicates whether the UE supports asynchronous DAPS handover in source PCell and inter-frequency target PCell.  | - |
| ***interFreqBandList***One entry corresponding to each supported E‑UTRA band listed in the same order as in *supportedBandListEUTRA*. | - |
| ***interFreqDAPS***Indicates whether the UE supports DAPS handover in source PCell and inter-frequency target PCell, i.e. support of simultaneous DL reception of PDCCH and PDSCH from source and target cell. For a BC, the capability applies to every carrier pair for source and target. A UE indicating this capability shall also support synchronous DAPS handover, and single UL transmission for inter-frequency DAPS handover. | - |
| ***interFreqMultiUL-TransmissionDAPS***Indicates that the UE supports simultaneous UL transmission in source PCell and inter-frequency target PCell. | - |
| ***interFreqNeedForGaps***Indicates need for measurement gaps when operating on the E‑UTRA band given by the entry in *bandListEUTRA* or on the E-UTRA band combination given by the entry in *bandCombinationListEUTRA* and measuring on the E‑UTRA band given by the entry in *interFreqBandList*. | - |
| ***interFreqProximityIndication***Indicates whether the UE supports proximity indication for inter-frequency E-UTRAN CSG member cells*.* | - |
| ***interFreqRSTD-Measurement***Indicates whether the UE supports inter-frequency RSTD measurements for OTDOA positioning, as specified in TS 36.355 [54]. | Yes |
| ***interFreqSI-AcquisitionForHO***Indicates whether the UE supports, upon configuration of si-RequestForHO by the network, acquisition and reporting of relevant information using autonomous gaps by reading the SI from a neighbouring inter-frequency cell. | Yes |
| ***interRAT-BandList***One entry corresponding to each supported band of another RAT listed in the same order as in the *interRAT-Parameters*. The NR bands reported in *SupportedBandListNR* are excluded from this list. | - |
| ***interRAT-BandListNR-EN-DC***One entry corresponding to each supported NR band listed in the same order as in the *supportedBandListEN-DC-r15*. If both *interRAT-BandListNR-EN-DC* and *interRAT-BandListNR-SA* are included, the UE shall set the same *interRAT-NeedForGapsNR* value and same *interRAT-NeedForInterruptionNR* value (if any) for the same NR band. | - |
| ***interRAT-BandListNR-SA***One entry corresponding to each supported NR band listed in the same order as in the *supportedBandListNR-SA*. If both *interRAT-BandListNR-EN-DC* and *interRAT-BandListNR-SA* are included, the UE shall set the same *interRAT-NeedForGapsNR* value and same *interRAT-NeedForInterruptionNR* value (if any) for the same NR band. | - |
| ***interRAT-enhancementNR***Indicates whether the UE supports enhanced inter-RAT NR measurement requirements to support high speed up to 500 km/h as specified in TS 36.133 [16], when EN-DC is not configured and when EN-DC is configured. | - |
| ***interRAT-NeedForGaps***Indicates need for DL measurement gaps when operating on the E‑UTRA band given by the entry in *bandListEUTRA or on the E-UTRA band combination given by the entry in bandCombinationListEUTRA* and measuring on the inter-RAT band given by the entry in the *interRAT-BandList*. | - |
| ***interRAT-NeedForGapsNR***Indicates need for measurement gaps when operating on the E‑UTRA band given by the entry in *supportedBandListEUTRA or on the E-UTRA band combination given by the entry in supportedBandCombination-r10 or supportedBandCombinationAdd-r11* or *supportedBandCombinationReduced-r13* and measuring on the NR band given by the entry in the *InterRAT-BandListNR*. | - |
| ***interRAT-NeedForInterruptionNR***Indicates need for interruption when operating on the E‑UTRA band given by the entry in *supportedBandListEUTRA* or on the E-UTRA band combination given by the entry in *supportedBandCombination-r10* or *supportedBandCombinationAdd-r11* or *supportedBandCombinationReduced-r13* and measuring without measurement gaps on the NR band given by the entry in the *InterRAT-BandListNR*. | - |
| ***interRAT-ParametersWLAN***Indicates whether the UE supports WLAN measurements configured by *MeasObjectWLAN* with corresponding quantity and report configuration in the supported WLAN bands. | - |
| ***interRAT-PS-HO-ToGERAN***Indicates whether the UE supports inter-RAT PS handover to GERAN or not. | Yes |
| ***intraBandContiguousCC-InfoList***Indicates, per serving carrier of which the corresponding bandwidth class includes multiple serving carriers (i.e. bandwidth class B, C, D and so on), the maximum number of supported layers for spatial multiplexing in DL and the maximum number of CSI processes supported. The number of entries is equal to the number of component carriers in the corresponding bandwidth class. The UE shall support the setting indicated in each entry of the list regardless of the order of entries in the list.The UE shall include the field only if it supports 4-layer spatial multiplexing in transmission mode3/4 for a subset of component carriers in the corresponding bandwidth class, or if the maximum number of supported layers for at least one component carrier is higher than *supportedMIMO-CapabilityDL-r10* in the corresponding bandwidth class, or if the number of CSI processes for at least one component carrier is higher than *supportedCSI-Proc-r11* in the corresponding band.This field may also be included for bandwidth class A but in such a case without including any sub-fields in *IntraBandContiguousCC-Info-r12* (see NOTE 6). | - |
| ***intraFreqA3-CE-ModeA***Indicates whether the UE when operating in CE Mode A supports *eventA3* for intra-frequency neighbouring cells. | - |
| ***intraFreqA3-CE-ModeB***Indicates whether the UE when operating in CE Mode B supports *eventA3* for intra-frequency neighbouring cells. | - |
| ***intraFreq-CE-NeedForGaps***Indicates need for measurement gaps when operating in CE on the E‑UTRA band given by the entry in *supportedBandListEUTRA.* |  |
| ***intraFreqAsyncDAPS***Indicates whether the UE supports asynchronous DAPS handover in source PCell and intra-frequency target PCell.  | - |
| ***intraFreqDAPS***Indicates whether UE supports DAPS handover in source PCell and intra-frequency target PCell, i.e. support of simultaneous DL reception of PDCCH and PDSCH from source and target cell. A UE indicating this capability shall also support synchronous DAPS handover, and single UL transmission for intra-frequency DAPS handover. | - |
| ***intraFreqHO-CE-ModeA***Indicates whether the UE when operating in CE Mode A supports intra-frequency handover. | - |
| ***intraFreqHO-CE-ModeB***Indicates whether the UE when operating in CE Mode B supports intra-frequency handover. | - |
| ***intraFreqProximityIndication***Indicates whether the UE supports proximity indication for intra-frequency E-UTRAN CSG member cells. | - |
| ***intraFreqSI-AcquisitionForHO***Indicates whether the UE supports, upon configuration of si-RequestForHO by the network, acquisition and reporting of relevant information using autonomous gaps by reading the SI from a neighbouring intra-frequency cell. | Yes |
| ***intraFreqTwoTAGs-DAPS***Indicates whether the UE supports different timing advance groups in source PCell and intra-frequency target PCell. It is mandatory for *intraFreqDAPS* capable UE. | - |
| ***jointEHC-ROHC-Config***Indicates whether the UE supports simultaneous configuration of EHC and ROHC protocols for the same DRB. | No |
| ***k-Max (in MIMO-CA-ParametersPerBoBCPerTM)***If signalled, the field indicates for a particular transmission mode the maximum number of NZP CSI RS resource configurations supported within a CSI process applicable for the concerned band combination. | No |
| ***k-Max (in MIMO-UE-ParametersPerTM)***Indicates for a particular transmission mode the maximum number of NZP CSI RS resource configurations supported within a CSI process applicable for band combinations for which the concerned capabilities are not signalled. | Yes |
| ***laa-PUSCH-Mode1***Indicates whether the UE supports LAA PUSCH mode 1as defined in TS 36.213 [23]. | - |
| ***laa-PUSCH-Mode2***Indicates whether the UE supports LAA PUSCH mode 2as defined in TS 36.213 [23]*.* | - |
| ***laa-PUSCH-Mode3***Indicates whether the UE supports LAA PUSCH mode 3as defined in TS 36.213 [23]*.* | - |
| ***locationReport***Indicates whether the UE supports reporting of its geographical location information to eNB. | - |
| ***loggedMBSFNMeasurements***Indicates whether the UE supports logged measurements for MBSFN. A UE indicating support for logged measurements for MBSFN shall also indicate support for logged measurements in Idle mode. | - |
| ***loggedMeasBT***Indicates whether the UE supports Bluetooth measurements in RRC idle mode. | - |
| ***loggedMeasIdleEventL1***Indicates whether the UE supports event triggered logged measurements for *eventL1* in *camped normally* state. | - |
| ***loggedMeasIdleEventOutOfCoverage***Indicates whether the UE supports event triggered logged measurements for *outOfCoverage* in *any cell selection* state. | - |
| ***loggedMeasUnComBarPre***Indicates whether the UE supports uncompensated barometric pressure measurements in RRC\_IDLE mode. | - |
| ***loggedMeasurementsIdle***Indicates whether the UE supports logged measurements in Idle mode. | - |
| ***loggedMeasWLAN***Indicates whether the UE supports WLAN measurements in RRC idle mode. | - |
| ***logicalChannelSR-ProhibitTimer***Indicates whether the UE supports the *logicalChannelSR-ProhibitTimer* as defined in TS 36.321 [6]. | - |
| ***longDRX-Command***Indicates whether the UE supports Long DRX Command MAC Control Element. | - |
| ***lowerMSD-MRDC***Indicates whether the UE supports lower maximum sensitivity degradation when the band is the victim band with sensitivity degradation as specified in TS 38.101-3 [101]. | - |
| ***lwa***Indicates whether the UE supports LTE-WLAN Aggregation (LWA). The UE which supports LWA shall also indicate support of *interRAT-ParametersWLAN-r13*. | - |
| ***lwa-BufferSize***Indicates whether the UE supports the layer 2 buffer sizes for "with support for split bearers" as defined in Table 4.1-3 and 4.1A-3 of TS 36.306 [5] for LWA. | - |
| ***lwa-HO-WithoutWT-Change***Indicates whether the UE supports handover where LWA configuration is retained without WT change and using LWA end-marker for PDCP key change indication for LWA operation. | - |
| ***lwa-RLC-UM***Indicates whether the UE supports RLC UM for LWA bearer. | - |
| ***lwa-SplitBearer***Indicates whether the UE supports the split LWA bearer (as defined in TS 36.300 [9]). | - |
| ***lwa-UL***Indicates whether the UE supports UL transmission over WLAN for LWA bearer. | - |
| ***lwip***Indicates whether the UE supports LTE/WLAN Radio Level Integration with IPsec Tunnel (LWIP). The UE which supports LWIP shall also indicate support of *interRAT-ParametersWLAN-r13*. | - |
| ***lwip-Aggregation-DL, lwip-Aggregation-UL***Indicates whether the UE supports aggregation of LTE and WLAN over DL/UL LWIP. The UE that indicates support of LWIP aggregation over DL or UL shall also indicate support of *lwip*. | - |
| ***makeBeforeBreak***Indicates whether the UE supports intra-frequency Make-Before-Break handover, and whether the UE which indicates *dc-Parameters* supports intra-frequency Make-Before-Break SeNB change, as defined in TS 36.300 [9]. | - |
| ***measGapPatterns-NRonly***Indicates whether the UE supports gap patterns 2, 3 and 11 in LTE standalone when the frequencies to be measured within this measurement gap are all NR frequencies.  | No |
| ***measGapPatterns-NRonly-ENDC***Indicates whether the UE supports gap patterns 2, 3 and 11 in (NG)EN-DC when the frequencies to be measured within this measurement gap are all NR frequencies.  | No |
| ***maximumCCsRetrieval***Indicates whether UE supports reception of *requestedMaxCCsDL* and *requestedMaxCCsUL*. | - |
| ***maxLayersMIMO-Indication***Indicates whether the UE supports the network configuration of *maxLayersMIMO*. If the UE supports *fourLayerTM3-TM4* or *intraBandContiguousCC-InfoList* or *FeatureSetDL-PerCC* for MR-DC, UE supports the configuration of *maxLayersMIMO* for these cases regardless of indicating *maxLayersMIMO-Indication*. | - |
| ***maxLayersSlotOrSubslotPUSCH***Indicates the maxiumum number of layers for slot-PUSCH or subslot-PUSCH transmission. | Yes |
| ***maxNumberCCs-SPT***Indicates the maximum number of supported CCs for short processing time. The UE capability is reported per band combination. The reported number of carriers applies to all the FS-type(s) *frameStructureType-SPT-r15* supported in a given band combination. Absence of the field indicates that 0 number of CCs are supported for short processing time. | - |
| ***maxNumberDL-CCs, maxNumberUL-CCs***Indicates for each TTI combination "sTTI-SupportedCombinations", the maximum number of supported DL CCs/UL CCs for short TTI. Absence of the field indicates that 0 number of CCs are supported for short TTI. | - |
| ***maxNumberDecoding***Indicates the maximum number of blind decodes in UE-specific search space per UE in one subframe for CA with more than 5 CCs as defined in TS 36.213 [23] which is supported by the UE. The number of blind decodes supported by the UE is the field value \* 32. Only values 5 to 32 can be used in this version of the specification. | No |
| ***maxNumberEHC-Contexts***Defines the maximum number of Ethernet header compression contexts supported by the UE across all DRBs and across UE's EHC compressor and EHC decompressor. The indicated number defines the number of contexts in addition to CID = "all zeros" as specified in Annex A of TS 38.323 [83]. | No |
| ***maxNumberROHC-ContextSessions***Set to the maximum number of concurrently active ROHC contexts supported by the UE, excluding context sessions that leave all headers uncompressed. cs2 corresponds with 2 (context sessions), cs4 corresponds with 4 and so on. The network ignores this field if the UE supports none of the ROHC profiles in *supportedROHC-Profiles*. If the UE indicates both *maxNumberROHC-ContextSessions* and *maxNumberROHC-ContextSessions-r14*, same value shall be indicated. | - |
| ***maxNumberUpdatedCSI-Proc, maxNumberUpdatedCSI-Proc-SPT***Indicates the maximum number of CSI processes to be updated across CCs. | No |
| ***maxNumberUpdatedCSI-Proc-STTI-Comb77, maxNumberUpdatedCSI-Proc-STTI-Comb27, maxNumberUpdatedCSI-Proc-STTI-Comb22-Set1, maxNumberUpdatedCSI-Proc-STTI-Comb22-Set2***Indicates the maximum number of CSI processes to be updated across CCs. Comb77 is applicable for {slot, slot}, Comb27 for {subslot, slot}, Comb22-Set1 for{subslot, subslot} processing timeline set 1 and the Comb22-Set2 for {subslot, subslot} processing timeline set 2. |  |
| ***mbms-AsyncDC***Indicates whether the UE in RRC\_CONNECTED supports MBMS reception via MRB on a frequency indicated in an *MBMSInterestIndication* message, where (according to *supportedBandCombination*) the carriers that are or can be configured as serving cells in the MCG and the SCG are not synchronized. If this field is included, the UE shall also include *mbms-SCell* and *mbms-NonServingCell*. The field indicates that the UE supports the feature for xDD if *mbms-SCell* and *mbms-NonServingCell* are supported for xDD. | - |
| ***mbms-MaxBW***Indicates maximum supported bandwidth (T) for MBMS reception, see TS 36.213 [23]. clause 11.1. If the value is set to *implicitValue*, the corresponding value of T is calculated as specified in TS 36.213 [23], clause 11.1. If the value is set to *explicitValue*, the actual value of T = *explicitValue* \* 40 MHz. | - |
| ***mbms-NonServingCell***Indicates whether the UE in RRC\_CONNECTED supports MBMS reception via MRB on a frequency indicated in an *MBMSInterestIndication* message, where (according to *supportedBandCombination* and to network synchronization properties) a serving cell may be additionally configured. If this field is included, the UE shall also include the *mbms-SCell* field. | Yes |
| ***mbms-ScalingFactor1dot25, mbms-ScalingFactor7dot5***Indicates parameter A(1.25 / A(7.5, i.e., scaling factor for processing one unit of bandwidth corresponding to subcarrier spacing of 1.25 kHz / 7.5 kHz, with respect to one unit of bandwidth corresponding to subcarrier spacing of 15 kHz. See TS 36.213 [23], clause 11.1. This field is included only if *subcarrierSpacingMBMS-khz1dot25 / subcarrierSpacingMBMS-khz7dot5* is included. This field shall be included if *mbms-MaxBW* and *subcarrierSpacingMBMS-khz1dot25 / subcarrierSpacingMBMS-khz7dot5* are included. | - |
| ***mbms-ScalingFactor0dot37, mbms-ScalingFactor2dot5***Indicates parameter A(0.37 / A(2..5, i.e., scaling factor for processing one unit of bandwidth corresponding to subcarrier spacing of 0.37 kHz / 2.5 kHz, with respect to one unit of bandwidth corresponding to subcarrier spacing of 15 kHz. See TS 36.213 [23], clause 11.1. This field is included only if *fembmsMixedCell* or *fembmsDedicatedCell* is included. This field shall be included if *subcarrierSpacingMBMS-khz0dot37 / subcarrierSpacingMBMS-khz2dot5* is included for at least one E-UTRA band in *mbms-SupportedBandInfoList*. | - |
| ***mbms-SCell***Indicates whether the UE in RRC\_CONNECTED supports MBMS reception via MRB on a frequency indicated in an *MBMSInterestIndication* message, when an SCell is configured on that frequency (regardless of whether the SCell is activated or deactivated). | Yes |
| ***mbms-SupportedBandInfoList***One entry corresponding to each supported E-UTRA band listed in the same order as in *supportedBandListEUTRA*. This list is included only if *fembmsMixedCell* or *fembmsDedicatedCell* is included. If *mbms-SupportedBandInfoList-v1700* is included, the UE shall include the same number of entries, and listed in the same order, as in *mbms-SupportedBandInfoList-r16*. | - |
| ***mcgRLF-RecoveryViaSCG***Indicates whether the UE supports recovery from MCG RLF via split SRB1 (if supported) and via SRB3 (if supported). | - |
| ***measGapPatterns-NRonly***Indicates whether the UE supports gap patterns 2, 3 and 11 in LTE standalone when the frequencies to be measured within this measurement gap are all NR frequencies.  | No |
| ***measGapPatterns-NRonly-ENDC***Indicates whether the UE supports gap patterns 2, 3 and 11 in (NG)EN-DC when the frequencies to be measured within this measurement gap are all NR frequencies.  | No |
| ***measurementEnhancements***This field defines whether UE supports measurement enhancements in high speed scenario (350 km/h) as specified in TS 36.133 [16]. | - |
| ***measurementEnhancements2***This field defines whether UE supports measurement enhancements in high speed scenario (up to 500 km/h velocity) as specified in TS 36.133 [16]. | - |
| ***measurementEnhancementsSCell***This field defines whether UE supports SCell measurement enhancements in high speed scenario (350 km/h) as specified in TS 36.133 [16]. | - |
| ***measGapPatterns***Indicates whether the UE that supports NR supports gap patterns 4 to 11 in LTE standalone as specified in TS 36.133 [16], and for independent measurement gap configuration on FR1 and per-UE gap in (NG)EN-DC as specified in TS 38.133 [84]. The first/ leftmost bit covers pattern 4, and so on. Value 1 indicates that the UE supports the concerned gap pattern. | - |
| ***mfbi-UTRA***It indicates if the UE supports the signalling requirements of multiple radio frequency bands in a UTRA FDD cell, as defined in TS 25.307 [65]. | - |
| ***MIMO-BeamformedCapabilityList***A list of pairs of {k-Max, n-MaxList} values with the nth entry indicating the values that the UE supports for each CSI process in case n CSI processes would be configured. | No |
| ***MIMO-CapabilityDL***The number of supported layers for spatial multiplexing in DL. The field may be absent for category 0 and category 1 UE in which case the number of supported layers is 1. | - |
| ***MIMO-CapabilityUL***The number of supported layers for spatial multiplexing in UL. Absence of the field means that the number of supported layers is 1. | - |
| ***MIMO-CA-ParametersPerBoBC***A set of MIMO parameters provided per band of a band combination. In case a subfield is absent, the concerned capabilities are the same as indicated at the per UE level (i.e. by MIMO-UE-ParametersPerTM). | - |
| ***mimo-CBSR-AdvancedCSI***Indicates whether UE supports CBSR for advanced CSI reporting with and without amplitude restriction as defined in TS 36.213 [23], clause 7.2. | Yes |
| ***min-Proc-TimelineSubslot***Minimum processing timeline for subslot operation. The minimum processing timeline can belong to one of two sets of associated processing and maximum TA operation. The sets supported can be different for 1os CRS-based SPDCCH, 2os CRS-based SPDCCH and DMRS-based SPDCCH. The sequence applies to:1. 1os CRS based SPDCCH2. 2os CRS based SPDCCH3. DMRS based SPDCCH | - |
| ***modifiedMPR-Behavior***Field encoded as a bit map, where at least one bit N is set to "1" if UE supports modified MPR/A-MPR behaviour N, see TS 36.101 [42]. All remaining bits of the field are set to "0". The leading / leftmost bit (bit 0) corresponds to modified MPR/A-MPR behaviour 0, the next bit corresponds to modified MPR/A-MPR behaviour 1 and so on.Absence of this field means that UE does not support any modified MPR/A-MPR behaviour. | - |
| ***mpdcch-InLteControlRegionCE-ModeA,*** ***mpdcch-InLteControlRegionCE-ModeB***Indicates whether UE operating in CE mode A/B supports MPDCCH reception in LTE control channel region as specified in TS 36.211 [21]. | Yes |
| ***mpsPriorityIndication***Indicates whether the UE supports *mpsPriorityIndication* on release with redirect. | - |
| ***multiACK-CSI-reporting***Indicates whether the UE supports multi-cell HARQ ACK and periodic CSI reporting and SR on PUCCH format 3. | Yes |
| ***multiBandInfoReport***Indicates whether the UE supports the acquisition and reporting of multi band information for *reportCGI*. | - |
| ***multiClusterPUSCH-WithinCC*** | Yes |
| ***multiNS-Pmax***Indicates whether the UE supports the mechanisms defined for cells broadcasting *NS-PmaxList*. | - |
| ***multiNS-PmaxAerial***Indicates whether the UE supports the mechanisms defined for cells broadcasting *NS-PmaxListAerial* and *freqBandInfoAerial*. | - |
| ***multipleCellsMeasExtension***Indicates whether the UE supports *numberOfTriggeringCells* in the report configuration. | - |
| ***multipleTimingAdvance***Indicates whether the UE supports multiple timing advances for each band combination listed in *supportedBandCombination*. If the band combination comprised of more than one band entry (i.e., inter-band or intra-band non-contiguous band combination), the field indicates that the same or different timing advances on different band entries are supported. If the band combination comprised of one band entry (i.e., intra-band contiguous band combination), the field indicates that the same or different timing advances across component carriers of the band entry are supported. It is mandatory for UEs to support 2 TAGs for inter frequency DAPS handover. | - |
| ***multipleUplinkSPS***Indicates whether the UE supports multiple uplink SPS and reporting SPS assistance information. A UE indicating *multipleUplinkSPS* shall also support V2X communication via Uu, as defined in TS 36.300 [9]. | - |
| ***must-CapabilityPerBand***Indicates that UE supports MUST, as specified in 36.212 [22], clause 5.3.3.1, on the band in the band combination. | - |
| ***must-TM234-UpTo2Tx-r14***Indicates that the UE supports MUST operation for TM2/3/4 using up to 2Tx. | - |
| ***must-TM89-UpToOneInterferingLayer-r14***Indicates that the UE supports MUST operation for TM8/9 with assistance information for up to 1 interfering layer. | - |
| ***must-TM89-UpToThreeInterferingLayers-r14***Indicates that the UE supports MUST operation for TM8/9 with assistance information for up to 3 interfering layers. | - |
| ***must-TM10-UpToOneInterferingLayer-r14***Indicates that the UE supports MUST operation for TM10 with assistance information for up to 1 interfering layer. | - |
| ***must-TM10-UpToThreeInterferingLayers-r14***Indicates that the UE supports MUST operation for TM10 with assistance information for up to 3 interfering layers. | - |
| ***naics-Capability-List***Indicates that UE supports NAICS, i.e. receiving assistance information from serving cell and using it to cancel or suppress interference of neighbouring cell(s) for at least one band combination. If not present, UE does not support NAICS for any band combination. The field *numberOfNAICS-CapableCC* indicates the number of component carriers where the NAICS processing is supported and the field *numberOfAggregatedPRB* indicates the maximum aggregated bandwidth across these of component carriers (expressed as a number of PRBs) with the restriction that NAICS is only supported over the full carrier bandwidth. The UE shall indicate the combination of {*numberOfNAICS-CapableCC, numberOfNAICS-CapableCC*} for every supported *numberOfNAICS-CapableCC*, e.g. if a UE supports {x CC, y PRBs} and {x-n CC, y-m PRBs} where n>=1 and m>=0, the UE shall indicate both.- For *numberOfNAICS-CapableCC* = 1, UE signals one value for *numberOfAggregatedPRB* from the range {50, 75, 100};- For *numberOfNAICS-CapableCC* = 2, UE signals one value for *numberOfAggregatedPRB* from the range {50, 75, 100, 125, 150, 175, 200};- For *numberOfNAICS-CapableCC* = 3, UE signals one value for *numberOfAggregatedPRB* from the range {50, 75, 100, 125, 150, 175, 200, 225, 250, 275, 300};- For *numberOfNAICS-CapableCC* = 4, UE signals one value for *numberOfAggregatedPRB* from the range {50, 100, 150, 200, 250, 300, 350, 400};- For *numberOfNAICS-CapableCC* = 5, UE signals one value for *numberOfAggregatedPRB* from the range {50, 100, 150, 200, 250, 300, 350, 400, 450, 500}. | No |
| ***ncsg***Indicates whether the UE supports measurement NCSG Pattern Id 0, 1, 2 and 3, as specified in TS 36.133 [16]. If this field is included and the UE supports asynchronous DC, the UE shall support NCSG Pattern Id 0, 1, 2 and 3. If this field is included but the UE does not support asynchronous DC, only NCSG Pattern Id 0 and 1 shall be supported | No |
| ***ng-EN-DC***Indicates whether the UE supports NGEN-DC. | - |
| ***n-MaxList (in MIMO-UE-ParametersPerTM)***Indicates for a particular transmission mode the maximum number of NZP CSI RS ports supported within a CSI process applicable for band combinations for which the concerned capabilities are not signalled. For *k-Max* values exceeding 1, the UE shall include the field and signal *k-Max* minus 1 bits. The first bit indicates *n-Max2*, with value 0 indicating 8 and value 1 indicating 16. The second bit indicates *n-Max3*, with value 0 indicating 8 and value 1 indicating 16. The third bit indicates *n-Max4*, with value 0 indicating 8 and value 1 indicating 32. The fourth bit indicates *n-Max5*, with value 0 indicating 16 and value 1 indicating 32. The fifth bit indicates *n-Max6*, with value 0 indicating 16 and value 1 indicating 32. The sixt bit indicates *n-Max7*, with value 0 indicating 16 and value 1 indicating 32. The seventh bit indicates *n-Max8*, with value 0 indicating 16 and value 1 indicating 64. | Yes |
| ***n-MaxList (in MIMO-CA-ParametersPerBoBCPerTM)***If signalled, the field indicates for a particular transmission mode the maximum number of NZP CSI RS ports supported within a CSI process applicable for band the concerned combination. Further details are as indicated for *n-MaxList* in *MIMO-UE-ParametersPerTM*. | No |
| ***NonContiguousUL-RA-WithinCC-List***One entry corresponding to each supported E-UTRA band listed in the same order as in *supportedBandListEUTRA*. | No |
| ***nonPrecoded (in MIMO-UE-ParametersPerTM)***Indicates for a particular transmission mode the UE capabilities concerning non-precoded EBF/ FD-MIMO operation (class A) for band combinations for which the concerned capabilities are not signalled in *MIMO-CA-ParametersPerBoBCPerTM*, and the FD-MIMO processing capability condition as described in NOTE 8 is satisfied. | Yes |
| ***nonPrecoded (in MIMO-CA-ParametersPerBoBCPerTM)***If signalled, the field indicates for a particular transmission mode, the UE capabilities concerning non-precoded EBF/ FD-MIMO operation (class A) applicable for the concerned band combination. | - |
| ***nonUniformGap***Indicates whether the UE supports measurement non uniform Pattern Id 1, 2, 3 and 4 in LTE standalone as specified in TS 36.133 [16]. | No |
| ***noResourceRestrictionForTTIBundling***Indicate whether the UE supports TTI bundling operation without resource allocation restriction. | No |
| ***nonCSG-SI-Reporting***Indicates whether UE will report PLMN list from non-CSG cells. | - |
| ***nr-AutonomousGaps-ENDC-FR1***Indicates whether the UE supports, upon configuration of *useAutonomousGapsNR* by the network, acquisition of relevant information from a neighbouring NR cell by reading the SI of the neighbouring cell on FR1 using autonomous gaps and reporting the acquired information to the network when it is configured with (NG)EN-DC. | Yes |
| ***nr-AutonomousGaps-ENDC-FR2***Indicates whether the UE supports, upon configuration of *useAutonomousGapsNR* by the network, acquisition of relevant information from a neighbouring NR cell by reading the SI of the neighbouring cell on FR2 using autonomous gaps and reporting the acquired information to the network when it is configured with (NG)EN-DC. | Yes |
| ***nr-AutonomousGaps-FR1***Indicates whether the UE supports, upon configuration of *useAutonomousGapsNR* by the network, acquisition of relevant information from a neighbouring NR cell by reading the SI of the neighbouring cell on FR1 using autonomous gaps and reporting the acquired information to the network when it is not configured with (NG)EN-DC. | Yes |
| ***nr-AutonomousGaps-FR2***Indicates whether the UE supports, upon configuration of *useAutonomousGapsNR* by the network, acquisition of relevant information from a neighbouring NR cell by reading the SI of the neighbouring cell on FR2 using autonomous gaps and reporting the acquired information to the network when it is not configured with (NG)EN-DC. | Yes |
| ***nr-CellIndividualOffset***Indicates whether the UE supports use of cell specific offset for NR inter-RAT measurements. | No |
| ***nr-HO-ToEN-DC***Indicates whether the UE supports inter-RAT handover from NR to EN-DC while NR-DC or NE-DC is not configured. This field is mandatory present if EN-DC is supported. | - |
| ***nr-IdleInactiveBeamMeasFR1***Indicates whether the UE supports performing eNB-configured SSB-based beam level RRM measurements for configured NR FR1 carrier(s) in RRC\_IDLE and in RRC\_INACTIVE as specified in TS 36.306 [5], clause 4.3.6.46. | No |
| ***nr-IdleInactiveBeamMeasFR2***Indicates whether the UE supports performing eNB-configured SSB-based beam level RRM measurements for configured NR FR2 carrier(s) in RRC\_IDLE and in RRC\_INACTIVE as specified in TS 36.306 [5], clause 4.3.6.47. | No |
| ***nr-IdleInactiveMeasFR1***Indicates whether UE supports reporting measurements performed on NR FR1 carrier(s) during RRC\_IDLE and RRC\_INACTIVE. | No |
| ***nr-IdleInactiveMeasFR2***Indicates whether UE supports reporting measurements performed on NR FR2 carrier(s) during RRC\_IDLE and RRC\_INACTIVE. | No |
| ***nr-RSSI-ChannelOccupancyReporting***Indicates whether the UE supports performing measurements and reporting of RSSI and channel occupancy on the corresponding NR band. | - |
| ***ntn-Autonomous-GNSS-Fix***This field indicates whether the UE supports autonomous GNSS position fix in RRC\_CONNECTED. | - |
| ***ntn-Connectivity-EPC***Indicates whether the UE supports NTN access when connected to EPC. If the UE indicates this capability, the UE shall support all NTN essential features as specified in TS 36.306 [5]. | - |
| ***ntn-DCI-HarqDisableMultiTB-CE-ModeB***This field indicates whether the UE supports DCI-based HARQ feedback disabling for downlink transmission when HARQ feedback disabling per HARQ process for downlink transmission is not configured by RRC and the UE is operating in CE mode B and when configured with *ce-PDSCH-MultiTB-Config*. | - |
| ***ntn-DCI-HarqDisableSingleTB-CE-ModeB***This field indicates whether the UE supports DCI-based HARQ feedback disabling for downlink transmission when HARQ feedback disabling per HARQ process for downlink transmission is not configured by RRC and when the UE is operating in CE mode B. | - |
| ***ntn-EventA4BasedCHO***This field indicates whether the UE supports Event A4-based conditional handover, i.e., *CondEvent A4*. | - |
| ***ntn-GNSS-EnhScenarioSupport***This field indicates whether the UE supports GNSS measurement and UL transmission extension enhancements in RRC\_CONNECTED for only GSO or NGSO scenario. If this field is not included, the GNSS measurement and UL transmission extension enhancements in RRC\_CONNECTED that are indicated as supported are applicable for both GSO and NGSO scenario. | - |
| ***ntn-HarqEnhScenarioSupport***This field indicates whether the UE supports UL and DL HARQ process enhancements for only GSO or NGSO scenario. If this field is not included, the UL and DL HARQ process enhancements that are indicated as supported are applicable for both GSO and NGSO scenario. | - |
| ***ntn-LocationBasedCHO-EFC***This field indicates whether the UE supports location-based conditional handover for earth fixed cell, i.e., *CondEvent D1*. | - |
| ***ntn-LocationBasedCHO-EMC***This field indicates whether the UE supports location-based conditional handover for earth moving cell, i.e., *CondEvent D2*. | - |
| ***ntn-LocationBasedMeasTrigger-EFC***This field indicates whether the UE supports location-based measurement trigger in RRC\_CONNECTED in earth fixed cell. | - |
| ***ntn-LocationBasedMeasTrigger-EMC***This field indicates whether the UE supports location-based measurement trigger in RRC\_CONNECTED in earth moving cell. | - |
| ***ntn-OffsetTimingEnh***Indicates whether the UE supports timing relationship enhancement using *Differential Koffset* as specified in TS 36.321 [6] and TS 36.213 [23]. | - |
| ***ntn-OverriddenHarqDisableMultiTB-CE-ModeB***This field indicates whether the UE supports DCI-based HARQ feedback disabling for downlink transmission by overriding the RRC configuration when the UE is operating in CE mode B and when configured with *ce-PDSCH-MultiTB-Config*. | - |
| ***ntn-OverriddenHarqDisableSingleTB-CE-ModeB***This field indicates whether the UE supports DCI-based HARQ feedback disabling for downlink transmission by overriding the RRC configuration when the UE is operating in CE mode B. | - |
| ***ntn-PUR-TimerDelay***Indicates whether the UE supports delaying the start of the *pur-ResponseWindowTimer* for NTN, see TS 36.321 [6]. | - |
| ***ntn-MeasForNR***Indicates whether the UE supports the inter-RAT measurements for redirection and cell reselection from an E-UTRA terrestrial network cell to an NR NTN cell, see TS 36.304 [4]. | - |
| ***ntn-RRC-HarqDisableMultiTB-CE-ModeA***This field indicates whether the UE supports HARQ feedback disabling per HARQ process for downlink transmission by RRC configuration when the UE is operating in CE mode A and when configured with *ce-PDSCH-MultiTB-Config*. | - |
| ***ntn-RRC-HarqDisableMultiTB-CE-ModeB***This field indicates whether the UE supports HARQ feedback disabling per HARQ process for downlink transmission by RRC configuration when the UE is operating in CE mode B and when configured with *ce-PDSCH-MultiTB-Config*. | - |
| ***ntn-RRC-HarqDisableSingleTB-CE-ModeA***This field indicates whether the UE supports HARQ feedback disabling per HARQ process for downlink transmission by RRC configuration when the UE is operating in CE mode A. | - |
| ***ntn-RRC-HarqDisableSingleTB-CE-ModeB***This field indicates whether the UE supports HARQ feedback disabling per HARQ process for downlink transmission by RRC configuration when the UE is operating in CE mode B. | - |
| ***ntn-SegmentedPrecompensationGaps***Indicates the minumum supported gap length between segments for segmented uplink transmission. Value *sym1* corresponds to 1 symbol, value *sl1* corresponds to 1 slot, value *sf1* corresponds to 1 subframe. | - |
| ***ntn-ScenarioSupport***Indicates whether the UE supports NTN features only for GSO or NGSO scenario. If a UE does not include this field but includes *ntn-Connectivity-EPC-r17*, the UE supports the NTN features for both GSO and NGSO scenarios. | - |
| ***ntn-SemiStaticHarqDisableSPS***This field indicates whether the UE supports HARQ feedback transmission for the first SPS PDSCH transmission after activation when the UE is operating in CE mode A. | - |
| ***ntn-TA-report***Indicates whether the UE supports timing advance reporting in RRC\_CONNECTED, see TS 36.321 [6]. | - |
| ***ntn-TimeBasedCHO***This field indicates whether the UE supports time-based conditional handover, i.e., *CondEvent T1*. | - |
| ***ntn-TimeBasedMeasTrigger***This field indicates whether the UE supports time-based measurement trigger in RRC\_CONNECTED. | - |
| ***ntn-Triggered-GNSS-Fix***This field indicates whether the UE supports network triggered GNSS position fix in RRC\_CONNECTED.  | - |
| ***ntn-UplinkHarq-ModeB-MultiTB***This field indicates whether the UE supports HARQ Mode B when scheduled with uplink transmission of multiple TBs. For BL UE or UE in CE, this field also indicates whether the UE supports the corresponding LCP restrictions for uplink transmission. | - |
| ***ntn-UplinkHarq-ModeB-SingleTB***This field indicates whether the UE supports HARQ Mode B. For BL UE or UE in CE, this field also indicates whether the UE supports the corresponding LCP restrictions for uplink transmission. | - |
| ***ntn-UplinkTxExtension***This field indicates whether the UE supports to perform UL transmission in a duration after original GNSS validity duration expires without GNSS re-acquisition. | - |
| ***numberOfBlindDecodesUSS***Indicates the maximum number of blind decodes in UE specific search space in one subframe for CCs configured with sTTI operation supported by the UE. The number of blind decodes supported by the UE is the field value X\*68. Field value ranges from 4 to 32. | Yes |
| ***nzp-CSI-RS-AperiodicInfo***Indicates whether the UE supports aperiodic NZP CSI-RS transmission for the indicated transmission mode. | Yes |
| ***nzp-CSI-RS-PeriodicInfo***Indicates whether the UE supports periodic NZP CSI-RS transmission for the indicated transmission mode. | Yes |
| ***otdoa-UE-Assisted***Indicates whether the UE supports UE-assisted OTDOA positioning, as specified in TS 36.355 [54]. | Yes |
| ***outOfOrderDelivery***Same as "*outOfOrderDelivery*" defined in TS 38.306 [87]. | No |
| ***outOfSequenceGrantHandling***Indicates whether the UE supports PUSCH transmissions with out of sequence UL grants as defined in TS 36.213 [23]. This field can be included only if uplinkLAA is included. | - |
| ***overheatingInd***Indicates whether the UE supports overheating assistance information. | No |
| ***overheatingIndForSCG***Indicates whether the UE supports the inclusion of NR SCG reduced configuration in the overheating assistance information. The UE which indicates support of *overheatingIndForSCG* shall also indicate support of *overheatingInd*. | - |
| ***pdcch-CandidateReductions***Indicates whether the UE supports PDCCH candidate reduction on UE specific search space as specified in TS 36.213 [23], clause 9.1.1. | No |
| ***pdcp-Duplication***Indicates whether the UE supports PDCP duplication. | - |
| ***pdcp-SN-Extension***Indicates whether the UE supports 15 bit length of PDCP sequence number. | - |
| ***pdcp-SN-Extension-18bits***Indicates whether the UE supports 18 bit length of PDCP sequence number. | - |
| ***pdcp-TransferSplitUL***Indicates whether the UE supports PDCP data transfer split in UL for the *drb-TypeSplit* as specified in TS 36.323 [8]. | - |
| ***pdcp-VersionChangeWithoutHO***Indicates whether, the UE supports changing the PDCP version of DRBs, from LTE PDCP to NR PDCP and vice versa, with and without handover. A UE supporting PDCP version change shall signal field *pdcp-Parameters-v1610*. When the field *pdcp-VersionChangeWithoutHO* is not included and *pdcp-Parameters-v1610* is included, it implies the UE supports PDCP version change only with handover. | - |
| ***pdsch-CollisionHandling***Indicates whether the UE supports PDSCH collision handling as specified in TS 36.213 [23].  | No |
| ***pdsch-InLteControlRegionCE-ModeA, pdsch-InLteControlRegionCE-ModeB***Indicates whether UE operating in CE mode A/B supports PDSCH reception in LTE control channel region as specified in TS 36.211 [21]. | Yes |
| ***pdsch-MultiTB-CE-ModeA, pdsch-MultiTB-CE-ModeB***Indicates whether the UE supports multiple TB scheduling in connected mode for PDSCH when operating in CE mode A/B, as specified in TS 36.211 [21] and TS 36.213 [23]. | Yes |
| ***pdsch-RepSubframe***Indicates whether the UE supports subframe PDSCH repetition. | Yes |
| ***pdsch-RepSlot***Indicates whether the UE supports slot PDSCH repetition. | Yes |
| ***pdsch-RepSubslot***Indicates whether the UE supports subslot PDSCH repetition. This field is only applicable for UEs supporting FDD. | - |
| ***pdsch-SlotSubslotPDSCH-Decoding***Indicates whether the UE supports decoding of PDSCH and slot-PDSCH/subslot-PDSCH assigned with C-RNTI/SPS C-RNTI in the same subframe for a given carrier. | Yes |
| ***perServingCellMeasurementGap***Indicates whether the UE supports per serving cell measurement gap indication, as specified in TS 36.133 [16]. | - |
| ***phy-TDD-ReConfig-FDD-PCell***Indicates whether the UE supports TDD UL/DL reconfiguration for TDD serving cell(s) via monitoring PDCCH with eIMTA-RNTI on a FDD PCell, and HARQ feedback according to UL and DL HARQ reference configurations. This bit can only be set to supported only if the UE supports FDD PCell and *phy-TDD-ReConfig-TDD-PCell* is set to supported. | No |
| ***phy-TDD-ReConfig-TDD-PCell***Indicates whether the UE supports TDD UL/DL reconfiguration for TDD serving cell(s) via monitoring PDCCH with eIMTA-RNTI on a TDD PCell, and HARQ feedback according to UL and DL HARQ reference configurations, and PUCCH format 3. | Yes |
| ***pmch-Bandwidth-n40, pmch-Bandwidth-n35, pmch-Bandwidth-n30***Indicates, for the E‑UTRA band corresponding to the entry in *mbms-SupportedBandInfoList-v1700*, whether the UE in RRC\_CONNECTED supports MBMS reception via MBSFN from MBMS-dedicated cells in an MBSFN area with PMCH bandwidth of 40/ 35/ 30 PRBs as described in TS 36.211 [21] and TS 36.213 [23]. | - |
| ***pmi-Disabling*** | Yes |
| ***powerClass-14dBm***Indicates whether the UE supports power class 14 dBm when operating in CE mode A or B for all the bands that are supported by the UE, as specified in TS 36.101 [42]. | - |
| ***powerPrefInd***Indicates whether the UE supports power preference indication. | No |
| ***powerUCI-SlotPUSCH, powerUCI-SubslotPUSCH***Indicates whether the UE supports BPRE derivation based on the actual derived O\_CQI. The parameter *uplinkPower-CSIPayload* configures the UE to derive BPRE based on either the actual value of O\_CQI or the largest value of O\_CQI across all RI values. If the UE does not support the capability, the UE will derive BPRE based on the largest value of O\_CQI across all RI values. | Yes |
| ***prach-Enhancements***This field defines whether the UE supports random access preambles generated from restricted set type B in high speed scenoario as specified in TS 36.211 [21]. | - |
| ***processingTimelineSet***Indicates, for each SPDCCH configuration, support for a set of TA values. Each set consists of two different processing timelines and associated maximum TA. Set 1 indicates support for n+4 and n+6 and set 2 indicates support for n+6 and n+8, see TS 36.211 [21], clause 8.1, The minimum processing timeline to use, out of the two options for a given set is configured by parameter *proc-Timeline*. Support of Set 1 implicitly means support of Set 2. | - |
| ***pucch-Format4***Indicates whether the UE supports PUCCH format 4. | Yes |
| ***pucch-Format5***Indicates whether the UE supports PUCCH format 5. | Yes |
| ***pucch-SCell***Indicates whether the UE supports PUCCH on SCell. | No |
| ***pur-CP-EPC-CE-ModeA, pur-CP-EPC-CE-ModeB, pur-CP-5GC-CE-ModeA, pur-CP-5GC-CE-ModeB***Indicates whether UE operating in CE mode A/B supports CP transmission using PUR when connected to EPC/ 5GC. | Yes |
| ***pur-CP-L1Ack***Indicates whether UE supports L1 acknowledgement in response to CP transmission using PUR when connected to EPC/ 5GC. | Yes |
| ***pur-FrequencyHopping***Indicates whether UE supports frequency hopping for transmission using PUR. | Yes |
| ***pur-PUSCH-NB-MaxTBS***Indicates whether the UE supports 2984 bits max UL TBS in 1.4 MHz for transmission using PUR when operating in CE mode A, as specified in TS 36.212 [22] and TS 36.213 [23]. | Yes |
| ***pur-RSRP-Validation***Indicates whether UE supports serving cell RSRP for TA validation for transmission using PUR when connected to EPC/ 5GC. | Yes |
| ***pur-SubPRB-CE-ModeA, pur-SubPRB-CE-ModeB***Indicates whether UE supports subPRB resource allocation for PUSCH for transmission using PUR when operating in CE mode A/B. | Yes |
| ***pur-UP-EPC-CE-ModeA, pur-UP-EPC-CE-ModeB, pur-UP-5GC-CE-ModeA, pur-UP-5GC-CE-ModeB***Indicates whether UE operating in CE mode A/B supports UP transmission using PUR when connected to EPC/ 5GC. | Yes |
| ***pusch-Enhancements***Indicates whether the UE supports the PUSCH enhancement mode as specified in TS 36.211 [21] and TS 36.213 [23]. | Yes |
| ***pusch-FeedbackMode***Indicates whether the UE supports PUSCH feedback mode 3-2. | No |
| ***pusch-MultiTB-CE-ModeA, pusch-MultiTB-CE-ModeB***Indicates whether the UE supports multiple TB scheduling in connected mode for PUSCH when operating in CE mode A/B, as specified in TS 36.211 [21] and TS 36.213 [23]. | Yes |
| ***pusch-SPS-MaxConfigSlot***Indicates the max number of SPS configurations across all cells for slot PUSCH. | Yes |
| ***pusch-SPS-MultiConfigSlot***Indicates the number of multiple SPS configurations of slot PUSCH for each serving cell. | Yes |
| ***pusch-SPS-MaxConfigSubframe***Indicates the max number of SPS configurations across all cells for subframe PUSCH. | Yes |
| ***pusch-SPS-MultiConfigSubframe***Indicates the number of multiple SPS configurations of subframe PUSCH for each serving cell. | Yes |
| ***pusch-SPS-MaxConfigSubslot***Indicates the max number of SPS configurations across all cells for subslot PUSCH. | - |
| ***pusch-SPS-MultiConfigSubslot***Indicates the number of multiple SPS configurations of subslot PUSCH for each serving cell. This field is only applicable for UEs supporting FDD. | - |
| ***pusch-SPS-SlotRepPCell***Indicates whether the UE supports SPS repetition for slot PUSCH for PCell. | Yes |
| ***pusch-SPS-SlotRepPSCell***Indicates whether the UE supports SPS repetition for slot PUSCH for PSCell. | Yes |
| ***pusch-SPS-SlotRepSCell***Indicates whether the UE supports SPS repetition for slot PUSCH for serving cells other than SpCell. | Yes |
| ***pusch-SPS-SubframeRepPCell***Indicates whether the UE supports SPS repetition for subframe PUSCH for PCell. | Yes |
| ***pusch-SPS-SubframeRepPSCell***Indicates whether the UE supports SPS repetition for subframe PUSCH for PSCell. | Yes |
| ***pusch-SPS-SubframeRepSCell***Indicates whether the UE supports SPS repetition for subframe PUSCH for serving cells other than SpCell. | Yes |
| ***pusch-SPS-SubslotRepPCell***Indicates whether the UE supports SPS repetition for subslot PUSCH for PCell. This field is only applicable for UEs supporting FDD. | - |
| ***pusch-SPS-SubslotRepPSCell***Indicates whether the UE supports SPS repetition for subslot PUSCH for PSCell. This field is only applicable for UEs supporting FDD. | - |
| ***pusch-SPS-SubslotRepSCell***Indicates whether the UE supports SPS repetition for subslot PUSCH for serving cells other than SpCell. This field is only applicable for UEs supporting FDD. | - |
| ***pusch-SRS-PowerControl-SubframeSet***Indicates whether the UE supports subframe set dependent UL power control for PUSCH and SRS. This field is only applicable for UEs supporting TDD. | Yes |
| ***qcl-CRI-BasedCSI-Reporting***Indicates whether the UE supports CRI based CSI feedback for the FeCoMP feature as specified in TS 36.213 [23], clause 7.1.10. | - |
| ***qcl-TypeC-Operation***The UE uses this field to indicate the support of all of the following three features: QCL Type-C operation for FeCoMP, the capability to support separate PDSCH RE mapping for different PDSCH CWs in non-coherent joint transmission and the capability to support handling new DMRS port to MIMO layer mapping for the CWs, as specified in TS 36.213 [23], clause 7.1.10. | - |
| ***qoe-MeasReport***Indicates whether the UE supports QoE Measurement Collection for streaming services. | - |
| ***qoe-MTSI-MeasReport***Indicates whether the UE supports QoE Measurement Collection for MTSI services. |  |
| ***rach-Less***Indicates whether the UE supports RACH-less handover, and whether the UE which indicates *dc-Parameters* supports RACH-less SeNB change, as defined in TS 36.300 [9]. | - |
| ***rach-Report***Indicates whether the UE supports delivery of *rach-Report.* | - |
| ***rach-ReportForNR***Indicates whether the UE supports NR RACH report in LTE, upon request from the network*.* | - |
| ***rai-Support***Defines whether the UE supports release assistance indication (RAI) as specified in TS 36.321 [6] for BL UEs. | No |
| ***rai-SupportEnh***Indicates whether the UE supports 2-bit RAI when connected to EPC as specified in TS 36.321 [6]. | - |
| ***rclwi***Indicates whether the UE supports RCLWI, i.e. reception of *rclwi-Configuration*. The UE which supports RLCWI shall also indicate support of *interRAT-ParametersWLAN-r13*. The UE which supports RCLWI and *wlan-IW-RAN-Rules* shall also support applying WLAN identifiers received in *rclwi-Configuration* for the access network selection and traffic steering rules when in RRC\_IDLE. | - |
| ***recommendedBitRate***Indicates whether the UE supports the bit rate recommendation message from the eNB to the UE as specified in TS 36.321 [6], clause 6.1.3.13*.* | No |
| ***recommendedBitRateMultiplier***Indicates whether the UE supports the bit rate multiplier for recommended bit rate MAC CE as specified in TS 36.321 [6], clause 6.1.3.13. If this field is included, the UE shall also include the *recommendedBitRate* field. | - |
| ***recommendedBitRateQuery***Indicates whether the UE supports the bit rate recommendation query message from the UE to the eNB as specified in TS 36.321 [6], clause 6.1.3.13. If this field is included, the UE shall also include the *recommendedBitRate* field. | No |
| ***reducedCP-Latency***Indicates whether the UE supports reduced CP latency. | Yes |
| ***reducedIntNonContComb***Indicates whether the UE supports receiving *requestReducedIntNonContComb* that requests the UE to exclude supported intra-band non-contiguous CA band combinations other than included in capability signalling as specified in TS 36.306 [5], clause 4.3.5.21. | - |
| ***reducedIntNonContCombRequested***Indicates that the UE excluded supported intra-band non-contiguous CA band combinations other than included in capability signalling as specified in TS 36.306 [5,] clause 4.3.5.21. | - |
| ***reflectiveQoS***Indicates whether the UE supports AS reflective QoS. | No |
| ***relWeightTwoLayers/ relWeightFourLayers/ relWeightEightLayers***Indicates relative weight of processing FD-MIMO with 2/ 4/ 8 layers with respect to non-FD-MIMO with the same number of layers, see NOTE 8. Value v1 corresponds to relative weight of 1, value v1dot25 corresponds to relative weight of 1.25 and so on. This field can be included only if the UE supports the corresponding number of layers (i.e., 2/ 4/ 8 layers). | - |
| ***reportCGI-NR-EN-DC***Indicates whether the UE supports Inter-RAT report CGI procedure towards NR cell when it is configured with (NG)EN-DC. | Yes |
| ***reportCGI-NR-NoEN-DC***Indicates whether the UE supports Inter-RAT report CGI procedure towards NR cell when it is not configured with (NG)EN-DC. | Yes |
| ***resumeWithMCG-SCellConfig***Indicates whether the UE supports (re-)configuration of E-UTRA MCG SCells. | - |
| ***resumeWithSCG-Config***Indicates whether the UE supports (re-)configuration of an NR SCG. | - |
| ***resumeWithStoredMCG-SCells***Indicates whether the UE supports not deleting the stored E-UTRA MCG SCell configuration when initiating the resume procedure. | - |
| ***resumeWithStoredSCG***Indicates whether the UE supports not deleting the stored NR SCG configuration when initiating the resume procedure. | - |
| ***srs-CapabilityPerBandPairList***Indicates, for a particular pair of bands, the SRS carrier switching parameters when switching between the band pair to transmit SRS on a PUSCH-less SCell as specified in TS 36.212 [22] and TS 36.213 [23]. If included, the UE shall include a number of entries as indicated in the following, and listed in the same order, as in *bandParameterList* for the concerned band combination:- For the first band, the UE shall include the same number of entries as in *bandParameterList* i.e. first entry corresponds to first band in *bandParameterList* and so on,- For the second band, the UE shall include one entry less i.e. first entry corresponds to the second band in *bandParameterList* and so on- And so on. | - |
| ***requestedBands***Indicates the frequency bands requested by E-UTRAN. | - |
| ***requestedCCsDL, requestedCCsUL***Indicates the maximum number of CCs requested by E-UTRAN. | - |
| ***requestedDiffFallbackCombList***Indicates the CA band combinations for which report of different UE capabilities is requested by E-UTRAN. | - |
| ***rf-RetuningTimeDL***Indicates the interruption time on DL reception within a band pair during the RF retuning for switching between the band pair to transmit SRS on a PUSCH-less SCell. n0 represents 0 OFDM symbols, n0dot5 represents 0.5 OFDM symbols, n1 represents 1 OFDM symbol and so on. This field is mandatory present if switching between the band pair is supported. | - |
| ***rf-RetuningTimeUL***Indicates the interruption time on UL transmission within a band pair during the RF retuning for switching between the band pair to transmit SRS on a PUSCH-less SCell. n0 represents 0 OFDM symbols, n0dot5 represents 0.5 OFDM symbols, n1 represents 1 OFDM symbol and so on. This field is mandatory present if switching between the band pair is supported. | - |
| ***rlc-AM-Ooo-Delivery***Indicates whether the UE supports out-of-order delivery from RLC to PDCP for RLC AM*.* | - |
| ***rlc-UM-Ooo-Delivery***Indicates whether the UE supports out-of-order delivery from RLC to PDCP for RLC UM*.* | - |
| ***rlm-ReportSupport***Indicates whether the UE supports RLM event and information reporting.  | - |
| ***rohc-ContextContinue***Same as "*continueROHC-Context*" defined in TS 38.306 [87]. | No |
| ***rohc-ContextMaxSessions***Same as "*maxNumberROHC-ContextSessions*" defined in TS 38.306 [87].  | No |
| ***rohc-Profiles***Same as "*supportedROHC-Profiles*" defined in TS 38.306 [87]. | No |
| ***rohc-ProfilesUL-Only***Same as "*uplinkOnlyROHC-Profiles*" defined in TS 38.306 [87]. | No |
| ***rsrqMeasWideband***Indicates whether the UE can perform RSRQ measurements with wider bandwidth. | Yes |
| ***rsrq-OnAllSymbols***Indicates whether the UE can perform RSRQ measurement on all OFDM symbols and also support the extended RSRQ upper value range from -3dB to 2.5dB in measurement configuration and reporting as specified in TS 36.133 [16]. | No |
| ***rs-SINR-Meas***Indicates whether the UE can perform RS-SINR measurements in RRC\_CONNECTED as specified in TS 36.214 [48]. | - |
| ***rssi-AndChannelOccupancyReporting***Indicates whether the UE supports performing measurements and reporting of RSSI and channel occupancy. This field can be included only if *downlinkLAA* is included. | - |
| ***sa-NR***Indicates whether the UE supports standalone NR as specified in TS 38.331 [82]. | No |
| ***satelliteInfoConfigDedicated***This field indicates whether the UE can be configured via dedicated signalling with NTN assistance information (i.e., *satelliteId-r18* or ephemeris information in *measObjectEUTRA*) to measure an NTN cell in RRC\_CONNECTED. | - |
| ***scalingFactorTxSidelink, scalingFactorRxSidelink***Indicates, for a particular band combination of EUTRA, the scaling facor, as defined in TS 38.306 [87], for the PC5 band combination(s) *v2x-SupportedBandCombinationListEUTRA-NR* on which the UE supports simultaneous transmission/reception of EUTRA and NR sidelink communication respectively, or simultaneous transmission or reception of EUTRA and joint V2X sidelink communication and NR sidelink communication respectively (as indicated by *v2x-SupportedTxBandCombListPerBC-v1630 /* *v2x-SupportedRxBandCombListPerBC-v1630*). The leading / leftmost value corresponds to the first band combination included in *v2x-SupportedBandCombinationListEUTRA-NR* which is indicated with value 1 by *v2x-SupportedTxBandCombListPerBC-v1630 /* *v2x-SupportedRxBandCombListPerBC-v1630*, the next value corresponds to the second band combination included in *v2x-SupportedBandCombinationListEUTRA-NR* which is indicated with value 1 by *v2x-SupportedTxBandCombListPerBC-v1630 /* *v2x-SupportedRxBandCombListPerBC-v1630* and so on. For each value of *ScalingFactorSidelink-r16*, value f0p4 indicates the scaling factor 0.4, f0p75 indicates 0.75, and so on. | - |
| ***scptm-AsyncDC***Indicates whether the UE in RRC\_CONNECTED supports MBMS reception via SC-MRB on a frequency indicated in an *MBMSInterestIndication* message, where (according to *supportedBandCombination*) the carriers that are or can be configured as serving cells in the MCG and the SCG are not synchronized. If this field is included, the UE shall also include *scptm-SCell* and *scptm-NonServingCell*. | Yes |
| ***scptm-NonServingCell***Indicates whether the UE in RRC\_CONNECTED supports MBMS reception via SC-MRB on a frequency indicated in an *MBMSInterestIndication* message, where (according to *supportedBandCombination* and to network synchronization properties) a serving cell may be additionally configured. If this field is included, the UE shall also include the *scptm-SCell* field. | Yes |
| ***scptm-Parameters***Presence of the field indicates that the UE supports SC-PTM reception as specified in TS 36.306 [5]. | Yes |
| ***scptm-SCell***Indicates whether the UE in RRC\_CONNECTED supports MBMS reception via SC-MRB on a frequency indicated in an *MBMSInterestIndication* message, when an SCell is configured on that frequency (regardless of whether the SCell is activated or deactivated). | Yes |
| ***scptm-ParallelReception***Indicates whether the UE in RRC\_CONNECTED supports parallel reception in the same subframe of DL-SCH transport blocks transmitted using C-RNTI/Semi-Persistent Scheduling C-RNTI and using SC-RNTI/G-RNTI as specified in TS 36.306 [5]. | Yes |
| ***secondSlotStartingPosition***Indicates whether the UE supports reception of subframes with second slot starting position as described in TS 36.211 [21] and TS 36.213 [23]. This field can be included only if *downlinkLAA* is included. | - |
| ***semiOL***Indicates whether the UE supports semi-open-loop transmission for the indicated transmission mode. | Yes |
| ***semiStaticCFI***Indicates whether the UE supports the semi-static configuration of CFI for subframe/slot/sub-slot operation.  | Yes |
| ***semiStaticCFI-Pattern***Indicates whether the UE supports the semi-static configuration of CFI pattern for subframe/slot/sub-slot operation. This field is only applicable for UEs supporting TDD. | - |
| ***sharedSpectrumMeasNR-EN-DC***Indicates whether the UE supports performing measurements and reporting of RSSI and channel occupancy on each supported NR band in EN-DC. If included, the UE shall include the same number of entries, and listed in the same order as in *supportedBandListEN-DC-r15*. | - |
| ***sharedSpectrumMeasNR-SA***Indicates whether the UE supports performing measurements and reporting of RSSI and channel occupancy on each supported NR band in NR SA. If included, the UE shall include the same number of entries, and listed in the same order as in *supportedBandListNR-SA-r15*. | - |
| ***shortCQI-ForSCellActivation***Indicates whether the UE supports additional CQI reporting periodicity after SCell activation. | Yes |
| ***shortMeasurementGap***Indicates whether the UE supports shorter measurement gap length (i.e. *gp2* and *gp3*) in LTE standalone as specified in TS 36.133 [16], and for independent measurement gap configuration on FR1 and per-UE gap in (NG)EN-DC as specified in TS38.133 [84]. | No |
| ***shortSPS-IntervalFDD***Indicates whether the UE supports uplink SPS intervals shorter than 10 subframes in FDD mode. | - |
| ***shortSPS-IntervalTDD***Indicates whether the UE supports uplink SPS intervals shorter than 10 subframes in TDD mode. | - |
| ***sigBasedEUTRA-LoggedMeasOverrideProtect***Indicates whether the UE supports the override protection of the signalling based logged measurements configured in E-UTRA when entering RRC\_CONNECTED state in NR. | - |
| ***simultaneousPUCCH-PUSCH***Indicates whether the UE supports simultaneous transmission of PUSCH/PUCCH and SlotOrSubslotPUSCH/SPUCCH (if supported). | Yes |
| ***simultaneousRx-Tx***Indicates whether the UE supports simultaneous reception and transmission on different bands for each band combination listed in *supportedBandCombination*. This field is only applicable for inter-band TDD band combinations. A UE indicating support of *simultaneousRx-Tx* and *dc-Support-r12* shall support different UL/DL configurations between PCell and PSCell. | - |
| ***simultaneousTx-DifferentTx-Duration***Indicates whether the UE supports simultaneous transmission of different transmission durations over different carriers. The different transmission durations can be of subframe, slot or subslot duration. | - |
| ***skipFallbackCombinations***Indicates whether UE supports receiving *requestSkipFallbackComb* that requests UE to exclude fallback band combinations from capability signalling. | - |
| ***skipFallbackCombRequested***Indicates whether *requestSkipFallbackComb* is requested by E-UTRAN. | - |
| ***skipMonitoringDCI-Format0-1A***Indicates whether UE supports blind decoding reduction on UE specific search space by not monitoring DCI Format 0 and 1A as specified in TS 36.213 [23], clause 9.1.1. | No |
| ***skipSubframeProcessing***This fields defines whether the UE supports aborting reception of PDSCH if the UE receives slot-PDSCH/subslot-PDSCH during an ongoing PDSCH reception and instead starts receiving the slot-PDSCH/subslot-PDSCH, as well as whether the UE supports aborting a PUSCH transmission if the UE gets a grant for a slot-PUSCH/ subslot-PUSCH transmission that overlaps with a grant received for a PUSCH transmission. The capability indicates the number of subframes that the UE may drop prior to the subframe in which it prioritizes the processing of slot/subslot PDSCH/PUSCH as described in TS 36.213 [23], clauses 7.1 and 8.0. Separate capability for UL and DL and per sTTI length in each direction*: skipProcessingDL-Slot, skipProcessingDL-Subslot, skipProcessingUL-Slot* and *skipProcessingUL-Subslot.* | - |
| ***skipUplinkDynamic***Indicates whether the UE supports skipping of UL transmission for an uplink grant indicated on PDCCH if no data is available for transmission as described in TS 36.321 [6]. | - |
| ***skipUplinkSPS***Indicates whether the UE supports skipping of UL transmission for a configured uplink grant if no data is available for transmission as described in TS 36.321 [6]. | - |
| ***sl-64QAM-Rx***Indicates whether the UE supports 64QAM for the reception of V2X sidelink communication. | - |
| ***sl-64QAM-Tx***Indicates whether the UE supports 64QAM for the transmission of V2X sidelink communication. | - |
| ***sl-A2X-Service***Indicates whether the UE supports A2X service and dedicated resource pool for A2X service. Value 'brid' indicates BRID is supported, value 'daa' indicates DAA is supported, and value 'bridAndDAA' indicates both are supported. | - |
| ***sl-CongestionControl***Indicates whether the UE supports Channel Busy Ratio measurement and reporting of Channel Busy Ratio measurement results to eNB for V2X sidelink communication. | - |
| ***sl-LowT2min***Indicates whether the UE supports 10ms as minimum value of T2 for resource selection procedure of V2X sidelink communication. | - |
| ***sl-ParameterNR***Includes the *SidelinkParametersNR* IE as specified in TS 38.331 [82]. The field includes the sidelink capability for NR-PC5, where *multipleSR-ConfigurationsSidelink,* *logicalChannelSR-DelayTimerSidelink* and *relayParameters* are not applicable. | - |
| ***sl-RateMatchingTBSScaling***Indicates whether the UE supports rate matching and TBS scalling for V2X sidelink communication. | - |
| ***slotPDSCH-TxDiv-TM8***Indicates whether the UE supports TX diversity transmission using ports 7 and 8 for TM8 for slot PDSCH. | - |
| ***slotPDSCH-TxDiv-TM9and10***Indicates whether the UE supports TX diversity transmission using ports 7 and 8 for TM9/10 for slot PDSCH. | Yes |
| ***slotSymbolResourceResvDL-CE-ModeA, slotSymbolResourceResvDL-CE-ModeB, slotSymbolResourceResvUL-CE-ModeA, slotSymbolResourceResvUL-CE-ModeB***Indicates whether the UE supports slot/symbol-level time-domain resource reservation in downlink/uplink when operating in CE mode A/B, as specified in TS 36.211 [21] and TS 36.213 [23]. | Yes |
| ***slss-SupportedTxFreq***Indicates whether the UE supports the SLSS transmission on single carrier or on multiple carriers in the case of sidelink carrier aggregation. | - |
| ***slss-TxRx***Indicates whether the UE supports SLSS/PSBCH transmission and reception in UE autonomous resource selection mode and eNB scheduled mode in a band for V2X sidelink communication. | - |
| ***sl-TxDiversity***Indicates whether the UE supports transmit diversity for V2X sidelink communication. See TS 36.101 [42]. | - |
| ***sn-SizeLo***Same as "*shortSN*" defined in TS 38.306 [87]. | No |
| ***spatialBundling-HARQ-ACK***Indicates whether UE supports HARQ-ACK spatial bundling on PUCCH or PUSCH as specified in TS 36.213 [23], clauses 7.3.1 and 7.3.2. | No |
| ***spdcch-differentRS-types***Indicates whether the UE supports monitoring of sPDCCH on RB sets with different RS types within a TTI. | Yes |
| ***spdcch-Reuse***Indicates whether the UE supports L1 based SPDCCH reuse. | Yes |
| ***sps-CyclicShift***Indicates whether the UE supports RRC configuration of cyclic shift for DMRS for UL SPS using 1ms TTI. | Yes |
| ***sps-ServingCell***Indicates whether the UE supports multiple UL/DL SPS configurations simultaneously active on different serving cells as specified in TS 36.321 [6]. | - |
| ***sps-STTI***Indicates whether the UE supports SPS in DL and/or UL for slot or subslot based PDSCH and PUSCH, respectively.  | Yes |
| ***srs-DCI7-TriggeringFS2***Indicates whether the UE supports SRS triggerring via DCI format 7 for FS2. | - |
| ***srs-Enhancements***Indicates whether the UE supports SRS enhancements. | Yes |
| ***srs-EnhancementsTDD***Indicates whether the UE supports TDD specific SRS enhancements. | Yes |
| ***srs-FlexibleTiming***Indicates whether the UE supports configuration of *soundingRS-FlexibleTiming-r14* for the corresponding band pair. For a TDD-TDD band pair, UE shall include at least one of *srs-FlexibleTiming* and/or *srs-HARQ-ReferenceConfig* when *rf-RetuningTimeDL* or *rf-RetuningTimeUL* corresponding to the band pair is larger than 1 OFDM symbol. | - |
| ***srs-HARQ-ReferenceConfig***Indicates whether the UE supports configuration of *harq-ReferenceConfig-r14* for the corresponding band pair. For a TDD-TDD band pair, UE shall include at least one of *srs-FlexibleTiming* and/or *srs-HARQ-ReferenceConfig* when *rf-RetuningTimeDL* or *rf-RetuningTimeUL* corresponding to the band pair is larger than 1 OFDM symbol. | - |
| ***srs-MaxSimultaneousCCs***Indicates the maximum number of simultaneously configurable target CCs for SRS switching (i.e., CCs for which srs-SwitchFromServCellIndex is configured) supported by the UE. | - |
| ***srs-UpPTS-6sym***Indicates whether the UE supports up to 6-symbol SRS in UpPTS. | - |
| ***srvcc-FromUTRA-FDD-ToGERAN***Indicates whether UE supports SRVCC handover from UTRA FDD PS HS to GERAN CS. | - |
| ***srvcc-FromUTRA-FDD-ToUTRA-FDD***Indicates whether UE supports SRVCC handover from UTRA FDD PS HS to UTRA FDD CS. | - |
| ***srvcc-FromUTRA-TDD128-ToGERAN***Indicates whether UE supports SRVCC handover from UTRA TDD 1.28Mcps PS HS to GERAN CS. | - |
| ***srvcc-FromUTRA-TDD128-ToUTRA-TDD128***Indicates whether UE supports SRVCC handover from UTRA TDD 1.28Mcps PS HS to UTRA TDD 1.28Mcps CS. | - |
| ***ss-CCH-InterfHandl***Indicates whether the UE supports synchronisation signal and common channel interference handling. | Yes |
| ***ss-SINR-Meas-NR-FR1, ss-SINR-Meas-NR-FR2***Indicates whether the UE can perform NR SS-SINR measurement for a frequency range (i.e. FR1 or FR2) as specified in TS 38.215 [89]. | - |
| ***ssp10-TDD-Only***Indicates the UE supports special subframe configuration 10 when operating only in TDD carriers (i.e., not in TDD/FDD CA or TDD/FS3 CA). A UE including this field shall not include *tdd-SpecialSubframe-r14*. | - |
| ***standaloneGNSS-Location***Indicates whether the UE is equipped with a standalone GNSS receiver that may be used to provide detailed location information in RRC measurement report and logged measurements. | - |
| ***sTTI-SPT-Supported***Indicates whether the UE supports the features STTI and/or SPT. If the UE supports STTI and/or SPT features, the UE shall report the field *sTTI-SPT-Supported* set to *supported* in capability signalling, irrespective of whether *requestSTTI-SPT-Capability* field is present or not. | - |
| ***sTTI-FD-MIMO-Coexistence***Indicates whether the UE supports CSI feedback for more than 8 NZP CSI-RS ports on subframe based PUSCH in any serving cell and supporting STTI in any serving cell. | - |
| ***sTTI-SupportedCombinations***Indicates the different combinations of short TTI lengths, see field description for *dl-STTI-Length* and *ul-STTI-Length*, that the UE supports in a single PUCCH group or in two PUCCH groups. A short TTI length combination is reported for DL first followed by UL. In case of two PUCCH groups the support for the primary PUCCH group is indicated first. | - |
| ***subcarrierPuncturingCE-ModeA, subcarrierPuncturingCE-ModeB***Indicates whether the UE supports subcarrier puncturing in downlink when operating in CE mode A/B, as specified in TS 36.211 [21] and TS 36.213 [23]. | Yes |
| ***subcarrierSpacingMBMS-khz7dot5, subcarrierSpacingMBMS-khz1dot25***Indicates the supported subcarrier spacings for MBSFN subframes in addition to 15 kHz subcarrier spacing. *subcarrierSpacingMBMS-khz1dot25* and *subcarrierSpacingMBMS-khz7dot5* indicates that the UE supports 1.25 and 7.5 kHz respectively for MBSFN subframes as described in TS 36.211 [21], clause 6.12. This field is included only if *fembmsMixedCell* or *fembmsDedicatedCell* is included. | - |
| ***subcarrierSpacingMBMS-khz2dot5, subcarrierSpacingMBMS-khz0dot37***Presence of this field indicates the supported subcarrier spacings of 2.5kHz / 0.37kHz for MBSFN subframes in addition to 15 kHz subcarrier spacing when operating on the E-UTRA band given by the entry in *mbms-SupportedBandInfoList* as described in TS 36.211 [21], clause 6.12. | - |
| ***subframeResourceResvDL-CE-ModeA, subframeResourceResvDL-CE-ModeB, subframeResourceResvUL-CE-ModeA, subframeResourceResvUL-CE-ModeB***Indicates whether the UE supports Subframe-level time-domain resource reservation in downlink/uplink when operating in CE mode A/B, as specified in TS 36.211 [21] and TS 36.213 [23]. | Yes |
| ***subslotPDSCH-TxDiv-TM9and10***Indicates whether the UE supports TX diversity transmission using ports 7 and 8 for TM9/10 for subslot PDSCH. | Yes |
| ***supportedBandCombination***Includes the supported CA band combinations, if any, and may include all the supported non-CA bands. | - |
| ***supportedBandCombinationAdd-r11***Includes additional supported CA band combinations in case maximum number of CA band combinations of *supportedBandCombination* is exceeded. | - |
| ***SupportedBandCombinationAdd-v11d0,*** ***SupportedBandCombinationAdd-v1250,*** ***SupportedBandCombinationAdd-v1270, SupportedBandCombinationAdd-v1320, SupportedBandCombinationAdd-v1380, SupportedBandCombinationAdd-v1390, SupportedBandCombinationAdd-v1430, SupportedBandCombinationAdd-v1450, SupportedBandCombinationAdd-v1470, SupportedBandCombinationAdd-v14b0, SupportedBandCombinationAdd-v1530, SupportedBandCombinationAdd-v1630, SupportedBandCombinationAdd-v1800***If included, the UE shall include the same number of entries, and listed in the same order, as in *SupportedBandCombinationAdd-r11*. | - |
| ***SupportedBandCombinationAdd-v1610***If included, the UE shall include the same number of entries, and listed in the same order, as in *SupportedBandCombinationAdd-r11*. If absent, network assumes gap is required when measurement is performed on any NR bands while UE is served by cell(s) belongs to an E-UTRA CA band combinations listed in *SupportedBandCombinationAdd-r11* except for the FR2 inter-RAT measurement which depends on the support of *independentGapConfig.* | - |
| ***SupportedBandCombinationExt, SupportedBandCombination-v1090, SupportedBandCombination-v10i0, SupportedBandCombination-v1130, SupportedBandCombination-v1250, SupportedBandCombination-v1270, SupportedBandCombination-v1320, SupportedBandCombination-v1380, SupportedBandCombination-v1390, SupportedBandCombination-v1430, SupportedBandCombination-v1450, SupportedBandCombination-v1470, SupportedBandCombination-v14b0, SupportedBandCombination-v1530, SupportedBandCombination-v1630, SupportedBandCombination-v1800***If included, the UE shall include the same number of entries, and listed in the same order, as in *supportedBandCombination-r10*. | - |
| ***SupportedBandCombination-v1610***If included, the UE shall include the same number of entries, and listed in the same order, as in *supportedBandCombination-r10*. If absent, network assumes gap is required when measurement is performed on any NR bands while UE is served by cell(s) belongs to an E-UTRA CA band combinations listed in *supportedBandCombination-r10* except for the FR2 inter-RAT measurement which depends on the support of *independentGapConfig.* | - |
| ***supportedBandCombinationReduced***Includes the supported CA band combinations, and may include the fallback CA combinations specified in TS 36.101 [42], clause 4.3A. This field also indicates whether the UE supports reception of *requestReducedFormat*. | - |
| ***SupportedBandCombinationReduced-v1320, SupportedBandCombinationReduced-v1380, SupportedBandCombinationReduced-v1390, SupportedBandCombinationReduced-v1430, SupportedBandCombinationReduced-v1450, SupportedBandCombinationReduced-v1470, SupportedBandCombinationReduced-v14b0, SupportedBandCombinationReduced-v1530, SupportedBandCombinationReduced-v1630, SupportedBandCombinationReduced-v1800***If included, the UE shall include the same number of entries, and listed in the same order, as in *supportedBandCombinationReduced-r13*. | - |
| ***SupportedBandCombinationReduced-v1610***If included, the UE shall include the same number of entries, and listed in the same order, as in *supportedBandCombinationReduced-r13*. If absent, network assumes gap is required when measurement is performed on any NR bands while UE is served by cell(s) belongs to an E-UTRA CA band combinations listed in *supportedBandCombinationReduced-r13* except for the FR2 inter-RAT measurement which depends on the support of *independentGapConfig.* | - |
| ***SupportedBandGERAN***GERAN band as defined in TS 45.005 [20]. | No |
| ***SupportedBandList1XRTT***One entry corresponding to each supported CDMA2000 1xRTT band class. | - |
| ***SupportedBandListEUTRA***Includes the supported E-UTRA bands. This field shall include all bands which are indicated in *BandCombinationParameters*. | - |
| ***SupportedBandListEUTRA-v9e0, SupportedBandListEUTRA-v1250, SupportedBandListEUTRA-v1310, SupportedBandListEUTRA-v1320***If included, the UE shall include the same number of entries, and listed in the same order, as in *supportedBandListEUTRA* (i.e. without suffix). | - |
| ***SupportedBandListGERAN*** | No |
| ***SupportedBandListHRPD***One entry corresponding to each supported CDMA2000 HRPD band class. | - |
| ***SupportedBandListNR-SA***Includes the NR bands supported by the UE in NR-SA (for handover and redirection). The field is included in case the UE supports NR SA as specified in TS 38.331 [32] and not otherwise. The presence of this field also indicates that the UE can perform both NR SS-RSRP and SS-RSRQ measurement in the included NR band(s) as specified in TS 38.215 [89]. | No |
| ***supportedBandListEN-DC***Includes the NR bands supported by the UE in (NG)EN-DC. The field is included in case the parameter *en-DC* or *ng-EN-DC* is present and set to *supported* and not otherwise. The presence of this field also indicates that the UE can perform both NR SS-RSRP and SS-RSRQ measurement in the included NR band(s) as specified in TS 38.215 [89]. | - |
| ***supportedBandListWLAN***Indicates the supported WLAN bands by the UE. | - |
| ***SupportedBandUTRA-FDD***UTRA band as defined in TS 25.101 [17]. | - |
| ***SupportedBandUTRA-TDD128***UTRA band as defined in TS 25.102 [18]. | - |
| ***SupportedBandUTRA-TDD384***UTRA band as defined in TS 25.102 [18]. | - |
| ***SupportedBandUTRA-TDD768***UTRA band as defined in TS 25.102 [18]. | - |
| ***supportedBandwidthCombinationSet***The *supportedBandwidthCombinationSet* indicated for a band combination is applicable to all bandwidth classes indicated by the UE in this band combination.Field encoded as a bit map, where bit N is set to "1" if UE support Bandwidth Combination Set N for this band combination, see 36.101 [42]. The leading / leftmost bit (bit 0) corresponds to the Bandwidth Combination Set 0, the next bit corresponds to the Bandwidth Combination Set 1 and so on. The UE shall neither include the field for a non-CA band combination, nor for a CA band combination for which the UE only supports Bandwidth Combination Set 0. | - |
| ***supportedCellGrouping***This field indicates for which mapping of serving cells to cell groups (i.e. MCG or SCG) the UE supports asynchronous DC. This field is only present for a band combination with more than two but less than six band entries where the UE supports asynchronous DC. If this field is not present but asynchronous operation is supported, the UE supports all possible mappings of serving cells to cell groups for the band combination. The bitmap size is selected based on the number of entries in the combinations, i.e., in case of three entries, the bitmap corresponding to *threeEntries* is selected and so on.A bit in the bit string set to 1 indicates that the UE supports asynchronous DC for the cell grouping option represented by the concerned bit position. Each bit position represents a different cell grouping option, as illustrated by a table, see NOTE 5. A cell grouping option is represented by a number of bits, each representing a particular band entry in the band combination with the left-most bit referring to the band listed first in the band combination, etc. Value 0 indicates that the carriers of the corresponding band entry are mapped to a first cell group, while value 1 indicates that the carriers of the corresponding band entry are mapped to a second cell group.It is noted that the mapping table does not include entries with all bits set to the same value (0 or 1) as this does not represent a DC scenario (i.e. indicating that the UE supports that all carriers of the corresponding band entry are in one cell group). | - |
| ***supportedCSI-Proc, sTTI-SupportedCSI-Proc***Indicates the maximum number of CSI processes supported on a component carrier within a band. Value n1 corresponds to 1 CSI process, value n3 corresponds to 3 CSI processes, and value n4 corresponds to 4 CSI processes. If this field is included, the UE shall include the same number of entries listed in the same order as in *BandParameters/STTI-SPT-BandParameters*. If the UE supports at least 1 CSI process on any component carrier, then the UE shall include this field in all bands in all band combinations. | - |
| ***supportedCSI-Proc (in FeatureSetDL-PerCC)***In MR-DC, indicates the number of CSI processes for the component carrier in the corresponding bandwidth class. If the UE supports at least 1 CSI process, then the UE shall include this field. | - |
| ***supportedMIMO-CapabilityDL-MRDC (in FeatureSetDL-PerCC)***In MR-DC, indicates the maximum number of supported layers in TM9/10 for the component carrier in the corresponding bandwidth class. | - |
| ***supportedNAICS-2CRS-AP***If included, the UE supports NAICS for the band combination. The UE shall include a bitmap of the same length, and in the same order, as in *naics-Capability-List,* to indicate 2 CRS AP NAICS capability of the band combination. The first/ leftmost bit points to the first entry of *naics-Capability-List*, the second bit points to the second entry of *naics-Capability-List*, and so on.For band combinations with a single component carrier, UE is only allowed to indicate {*numberOfNAICS-CapableCC*, *numberOfAggregatedPRB*} = {1, 100} if NAICS is supported. | - |
| ***supportedOperatorDic***Indicates whether the UE supports operator defined dictionary. If UE supports operator defined dictionary, the UE shall report *versionOfDictionary* and *associatedPLMN-ID* of the stored operator defined dictionary. This parameter is not required to be present if the UE is in VPLMN. In this release of the specification, UE can only support one operator defined dictionary. The *associatedPLMN-ID* is only associated to the operator defined dictionary which has no relationship with UE's HPLMN ID. | - |
| ***supportRohcContextContinue***Indicates whether the UE supports ROHC context continuation operation where the UE does not reset the current ROHC context upon handover. | - |
| ***supportedROHC-Profiles***Indicates the ROHC profiles that UE supports in both uplink and downlink. | - |
| ***supportedUplinkOnlyROHC-Profiles***Indicates the ROHC profiles that UE supports in uplink and not in downlink, see TS 36.323 [8] | - |
| ***supportedStandardDic***Indicates whether the UE supports standard dictionary for SIP and SDP as specified in TS 36.323 [8]. | - |
| ***supportedUDC***Indicates whether the UE supports UL data compression, see TS 36.323 [8]. | - |
| ***tdd-SpecialSubframe***Indicates whether the UE supports TDD special subframe defined in TS 36.211 [21]. A UE shall indicate *tdd-SpecialSubframe-r11* if it supports the TDD special subframes ssp7 and ssp9. A UE shall indicate *tdd-SpecialSubframe-r14* if it supports the TDD special subframe ssp10, except when *ssp10-TDD-Only-r14* is included. | Yes |
| ***tdd-FDD-CA-PCellDuplex***The presence of this field indicates that the UE supports TDD/FDD CA in any supported band combination including at least one FDD band with *bandParametersUL* and at least one TDD band with *bandParametersUL*. The first bit is set to "1" if UE supports the TDD PCell. The second bit is set to "1" if UE supports FDD PCell. This field is included only if the UE supports band combination including at least one FDD band with *bandParametersUL* and at least one TDD band with *bandParametersUL*. If this field is included, the UE shall set at least one of the bits as "1". If this field is included with DC, then it is applicable within a CG, and the presence of this field indicates the capability of the UE to support TDD/FDD CA with at least one FDD band and at least one TDD band in the same CG, with the value indicating the support for TDD/FDD PCell (PSCell). | No |
| ***tdd-TTI-Bundling***The presence of this field indicates whether the UE supporting TDD special subframe configuration 10 also supports TTI bundling for TDD configuration 2 and 3 when PUSCH transimission in UpPTS is configured, see TS 36.213 [23], clause 8.0. If this field is present, the *tdd-SpecialSubframe-r14* or *ssp10-TDD-Only-r14* shall be present. | Yes |
| ***timeReferenceProvision***Indicates whether the UE supports provision of time reference in *DLInformationTransfer* message. | - |
| ***timeSeparationSlot2, timeSeparationSlot4***Indicates whether the UE supports time staggering length of 2 slots (MBSFN reference signal pattern type 2) / 4 slots (MBSFN reference signal pattern type 1) for MBSFN-RS associated with PMCH with subcarrier spacing of 0.37 kHz for MBSFN subframes when operating on the E‑UTRA band given by the entry in *mbms-SupportedBandInfoList* as described in TS 36.211 [21], clause 6.10.2.2.4. | - |
| ***timerT312***Indicates whether the UE supports T312. | No |
| ***tm5-FDD***Indicates whether the UE supports the PDSCH transmission mode 5 in FDD. | - |
| ***tm5-TDD***Indicates whether the UE supports the PDSCH transmission mode 5 in TDD. | - |
| ***tm6-CE-ModeA***Indicates whether the UE supports tm6 operation in CE mode A, see TS 36.213 [23], clause 7.2.3. This field can be included only if *ce-ModeA* is included. | Yes |
| ***tm8-slotPDSCH***Indicates whether the UE supports configuration and decoding of TM8 for slot PDSCH in TDD. | - |
| ***tm9-CE-ModeA***Indicates whether the UE supports tm9 operation in CE mode A, see TS 36.213 [23], clause 7.2.3. This field can be included only if *ce-ModeA* is included. | Yes |
| ***tm9-CE-ModeB***Indicates whether the UE supports tm9 operation in CE mode B, see TS 36.213 [23], clause 7.2.3. This field can be included only if *ce-ModeB* is included. | Yes |
| ***tm9-LAA***Indicates whether the UE supports tm9 operation on LAA cell(s). This field can be included only if *downlinkLAA* is included. | - |
| ***tm9-slotSubslot***Indicates whether the UE supports configuration and decoding of TM9 for slot and/or subslot PDSCH for non-MBSFN. | Yes |
| ***tm9-slotSubslotMBSFN***Indicates whether the UE supports configuration and decoding of TM9 for slot and/or subslot PDSCH for MBSFN. | Yes |
| ***tm9-With-8Tx-FDD***Indicates whether the UE supports PDSCH transmission mode 9 with 8 CSI reference signal ports for FDD when not operating in CE mode. | Yes |
| ***tm10-LAA***Indicates whether the UE supports tm10 operation on LAA cell(s). This field can be included only if *downlinkLAA* is included. | - |
| ***tm10-slotSubslot***Indicates whether the UE supports configuration and decoding of TM10 for slot and/or subslot PDSCH for non-MBSFN. | Yes |
| ***tm10-slotSubslotMBSFN***Indicates whether the UE supports configuration and decoding of TM10 for slot and/or subslot PDSCH for MBSFN. | Yes |
| ***totalWeightedLayers***Indicates total number of weighted layers the UE can process for FD-MIMO. See NOTE 8. | - |
| ***twoAntennaPortsForPUCCH*** | No |
| ***twoStepSchedulingTimingInfo***Presence of this field indicates that the UE supports uplink scheduling using PUSCH trigger A and PUSCH trigger B (as defined in TS 36.213 [23]).This field also indicates the timing between the PUSCH trigger B and the earliest time the UE supports performing the associated UL transmission. For reception of PUSCH trigger B in subframe N, value *nPlus1* indicates that the UE supports performing the UL transmission in subframe N+1, value *nPlus2* indicates that the UE supports performing the UL transmission in subframe N+2, and so on.This field can be included only if *uplinkLAA* is included. | - |
| ***txAntennaSwitchDL, txAntennaSwitchUL***The presence of *txAntennaSwitchUL* indicates the UE supports transmit antenna selection for this UL band in the band combination as described in TS 36.213 [23], clauses 8.2 and 8.7.The field *txAntennaSwitchDL* indicates the entry number of the first-listed band with UL in the band combination that affects this DL. The field *txAntennaSwitchUL* indicates the entry number of the first-listed band with UL in the band combination that switches together with this UL. Value 1 means first entry, value 2 means second entry and so on. All DL and UL that switch together indicate the same entry number.For the case of carrier switching, the antenna switching capability for the target carrier configuration is indicated as follows:For UE configured with a set of component carriers belonging to a band combination Cbaseline = {b1(1),…,bx(1),…,by(0),…}, where "1/0" denotes whether the corresponding band has an uplink, if a component carrier in bx is to be switched to a component carrier in by (according to *srs-SwitchFromServCellIndex*), the antenna switching capability is derived based on band combination Ctarget = {b1(1),…,bx(0),…,by(1),…}. | - |
| ***txDiv-PUCCH1b-ChSelect***Indicates whether the UE supports transmit diversity for PUCCH format 1b with channel selection. | Yes |
| ***txDiv-SPUCCH***Indicates whether the UE supports Tx diversity on SPUCCH format 1/1a/1b/3. | Yes |
| ***tx-Sidelink, rx-Sidelink***Indicates that the UE supports sidelink transmission/reception on the band in the band combination.For NR sidelink transmission, *tx-Sidelink* is only applicable if the UE supports at least one of *sl-TransmissionMode1-r16* and *sl-TransmissionMode2-r16* on the band as specified in TS 38.331 [82].For NR sidelink reception, *rx-Sidelink* is only applicable if the UE supports *sl-Reception-r16* on the band as specified in TS 38.331 [82]. | - |
| ***uci-PUSCH-Ext***Indicates whether the UE supports an extension of UCI delivering more than 22 HARQ-ACK bits on PUSCH as specified in TS 36.212 [22], clause 5.2.2.6 and TS 36.213 [23], clause 8.6.3. | No |
| ***ue-AutonomousWithFullSensing***Indicates whether the UE supports transmitting PSCCH/PSSCH using UE autonomous resource selection mode with full sensing (i.e., continuous channel monitoring) for V2X sidelink communication and the UE supports maximum transmit power associated with Power class 3 V2X UE, see TS 36.101 [42]. | - |
| ***ue-AutonomousWithPartialSensing***Indicates whether the UE supports transmitting PSCCH/PSSCH using UE autonomous resource selection mode with partial sensing (i.e., channel monitoring in a limited set of subframes) for V2X sidelink communication and the UE supports maximum transmit power associated with Power class 3 V2X UE, see TS 36.101 [42]. | - |
| ***ue-Category***UE category as defined in TS 36.306 [5]. Set to values 1 to 12 in this version of the specification. | - |
| ***ue-CategoryDL***UE DL category as defined in TS 36.306 [5]. Value *n17* corresponds to UE category 17, value *m1* corresponds to UE category M1, value *oneBis* corresponds to UE category 1bis, value m2 corresponds to UE category M2. For ASN.1 compatibility, a UE indicating DL category 0, m1 or m2 shall also indicate any of the categories (1..5) in *ue-Category* (without suffix), which is ignored by the eNB, a UE indicating UE category oneBis shall also indicate UE category 1 in *ue-Category* (without suffix), and a UE indicating UE category m2 shall also indicate UE category m1. The field *ue-CategoryDL* is set to values 0, m1, oneBis, m2, 4, 6, 7, 9 to 16, n17, 18, 19, 20, 21, 22, 23, 24, 25, 26 in this version of the specification. | - |
| ***ue-CategorySL-C-TX***UE SL category for V2X transmission as defined in TS 36.306 [5]. Set to values 1 to 5 in this version of the specification. | - |
| ***ue-CategorySL-C-RX***UE SL category for V2X reception as defined in TS 36.306 [5]. Set to values 1 to 4 in this version of the specification. | - |
| ***ue-CategoryUL***UE UL category as defined in TS 36.306 [5]. Value *n14* corresponds to UE category 14, value *n16* corresponds to UE category 16 and so on. Value *m1* corresponds to UE category M1, value *m2* corresponds to UE category M2, value *oneBis* corresponds to UE category 1bis. The field *ue-CategoryUL* is set to values m1, m2, 0, oneBis, 3, 5, 7, 8, 13, n14, 15, n16 to n21 or 22 to 26 in this version of the specification. | - |
| ***ue-CA-PowerClass-N***Indicates whether the UE supports UE power class N in the E-UTRA band combination, see TS 36.101 [42] and TS 36.307 [78]. If *ue-CA-PowerClass-N* is not included, UE supports the default UE power class in the E-UTRA band combination, see TS 36.101 [42]. | - |
| ***ue-CE-NeedULGaps***Indicates whether the UE needs uplink gaps during continuous uplink transmission in FDD as specified in TS 36.211 [21] and TS 36.306 [5]. | - |
| ***ue-PowerClass-N, ue-PowerClass-5***Indicates whether the UE supports UE power class 1, 2, 4 or 5 in the E-UTRA band, see TS 36.101 [42] and TS 36.307 [79] and TS 36.102 [113] for NTN capable UE. UE includes either *ue-PowerClass-N* or *ue-PowerClass-5*. If neither *ue-PowerClass-N* nor *ue-PowerClass-5* is included, UE supports the default UE power class in the E-UTRA band, see TS 36.101 [42] and TS 36.102 [113] for NTN capable UE. | - |
| ***ue-Rx-TxTimeDiffMeasurements***Indicates whether the UE supports Rx - Tx time difference measurements. | No |
| ***ue-SpecificRefSigsSupported*** | No |
| ***ue-SSTD-Meas***Indicates whether the UE supports SSTD measurements between the PCell and the PSCell as specified in TS 36.214 [48] and TS 36.133 [16]. | - |
| ***ue-TxAntennaSelectionSupported***Except for the supported band combinations for which *bandParameterList-v1380* is included, TRUE indicates that the UE is capable of supporting UE transmit antenna selection such that all the supported bands in the band combination are affected by transmit antenna switching, as described in TS 36.213 [23], clause 8.7. E-UTRAN ignores this field for band combinations for which *bandParameterList-v1380* is included. | Yes |
| ***ue-TxAntennaSelection-SRS-1T4R***Indicates whether the UE supports selecting one antenna among four antennas to transmit SRS for the corresponding band of the band combination as described in TS 36.213 [23]. | - |
| ***ue-TxAntennaSelection-SRS-2T4R-2Pairs***Indicates whether the UE supports selecting one antenna pair between two antenna pairs to transmit SRS simultaneously for the corresponding band of the band combination as described in TS 36.213 [23]. | - |
| ***ue-TxAntennaSelection-SRS-2T4R-3Pairs***Indicates whether the UE supports selecting one antenna pair among three antenna pairs to transmit SRS simultaneously for the corresponding band of the band combination as described in TS 36.213 [23]. | - |
| ***ul-64QAM***Indicates whether the UE supports 64QAM in UL on the band. This field is only present when the field ue*-CategoryUL* indicates UL UE category that supports UL 64QAM, see TS 36.306 [5], Table 4.1A-2. If the field is present for one band, the field shall be present for all bands including downlink only bands. | - |
| ***ul-256QAM***Indicates whether the UE supports 256QAM in UL on the band in the band combination. This field is only present when the field ue*-CategoryUL* indicates UL UE category that supports 256QAM in UL, see TS 36.306 [5], Table 4.1A-2. The UE includes this field only if the field *ul-256QAM-perCC-InfoLis*t is not included. | - |
| ***ul-256QAM (in FeatureSetUL-PerCC)***Indicates whether the UE supports 256QAM in UL for MR-DC within the indicated feature set. This field is only present when the field ue-CategoryUL indicates UL UE category that supports 256QAM in UL, see TS 36.306 [5], Table 4.1A-2. | - |
| ***ul-256QAM-perCC-InfoList***Indicates, per serving carrier of which the corresponding bandwidth class includes multiple serving carriers (i.e. bandwidth class B, C, D and so on), whether the UE supports 256QAM in the band combination. The number of entries is equal to the number of component carriers in the corresponding bandwidth class. The UE shall support the setting indicated in each entry of the list regardless of the order of entries in the list. This field is only present when the field *ue-CategoryUL* indicates UL UE category that supports 256QAM in UL, see TS 36.306 [5], Table 4.1A-2. The UE includes this field only if the field *ul-256QAM* is not included. | - |
| ***ul-256QAM-Slot***Indicates whether the UE supports 256QAM in UL for slot TTI operation on the band.  | - |
| ***ul-256QAM-Subslot***Indicates whether the UE supports 256QAM in UL for subslot TTI operation on the band.  | - |
| ***ul-AsyncHarqSharingDiff-TTI-Lengths***Indicates whether the UE supports UL asynchronous HARQ sharing between different TTI lengths for an UL serving cell. | Yes |
| ***ul-CoMP***Indicates whether the UE supports UL Coordinated Multi-Point operation. | No |
| ***ul-dmrs-Enhancements***Indicates whether the UE supports UL DMRS enhancements as defined in TS 36.211 [21], clause 6.10.3A. | Yes |
| ***ul-PDCP-AvgDelay***Indicates whether the UE supports UL PDCP Packet Average Delay measurement (as specified in TS 38.314 [103]) and reporting in RRC\_CONNECTED. | - |
| ***ul-PDCP-Delay***Indicates whether the UE supports UL PDCP Packet Delay per QCI measurement as specified in TS 36.314 [71]. | - |
| ***ul-powerControlEnhancements***Indicates whether UE supports UplinkPowerControlDedicated. | Yes |
| ***ul-RRC-Segmentation***Indicates the UE supports uplink RRC segmentation of *UECapabilityInformation*. | - |
| ***uplinkLAA***Presence of the field indicates that the UE supports uplink LAA operation. | - |
| ***uss-BlindDecodingAdjustment***Indicates whether the UEsupports blind decoding adjustment on UE specific search space as defined in TS 36.213 [22]. This field can be included only if uplinkLAA is included. | - |
| ***uss-BlindDecodingReduction***Indicates whether the UE supports blind decoding reduction on UE specific search space by not monitoring DCI format 0A/0B/4A/4B as defined in TS 36.213 [22]. This field can be included only if uplinkLAA is included. | - |
| ***unicastFrequencyHopping***Indicates whether the UE supports frequency hopping for unicast MPDCCH/PDSCH (configured by *mpdcch-pdsch-HoppingConfig*) and unicast PUSCH (configured by *pusch-HoppingConfig*). | - |
| ***unicast-fembmsMixedSCell***Indicates whether the UE supports unicast reception from FeMBMS/Unicast mixed cell. This field is included only if UE supports carrier aggregation. | No |
| ***utra-GERAN-CGI-Reporting-ENDC***Indicates whether the UE supports Inter-RAT report CGI procedure towards GERAN/UTRA cell when it is configured with (NG)EN-DC wherein either MN and SN have different DRX cycles, or on-duration configured by MN does not contain on-duration configured by SN if their DRX cycles are same. | Yes |
| ***utran-ProximityIndication***Indicates whether the UE supports proximity indication for UTRAN CSG member cells. | - |
| ***utran-SI-AcquisitionForHO***Indicates whether the UE supports, upon configuration of si-RequestForHO by the network, acquisition and reporting of relevant information using autonomous gaps by reading the SI from a neighbouring UMTS cell. | Yes |
| ***v2x-BandParametersNR***Includes the NR *BandParametersSidelink-r16* IE as specified in TS 38.331 [82]. The field includes the per-band per-band-combination sidelink capability for NR-PC5. | - |
| ***v2x-BandParametersEUTRA-NR-v1710***Includes the *BandParametersSidelinkEUTRA-NR-v1710* IE as specified in TS 38.331 [82]. The field includes the per-band per-band-combination sidelink capability for NR-PC5. | - |
| ***v2x-BandwidthClassTxSL, v2x-BandwidthClassRxSL***The bandwidth class for V2X sidelink transmission and reception supported by the UE as defined in TS 36.101 [42], Table 5.6G.1-3.The UE explicitly includes all the supported bandwidth class combinations for V2X sidelink transmission or reception in the band combination signalling. Support for one bandwidth class does not implicitly indicate support for another bandwidth class. | - |
| ***v2x-eNB-Scheduled***Indicates whether the UE supports transmitting PSCCH/PSSCH using dynamic scheduling, SPS in eNB scheduled mode for V2X sidelink communication, reporting SPS assistance information and the UE supports maximum transmit power associated with Power class 3 V2X UE, see TS 36.101 [42] in a band. | - |
| ***v2x-EnhancedHighReception***Indicates whether the UE supports reception of 30 PSCCH in a subframe and decoding of 204 RBs per subframe counting both PSCCH and PSSCH in a band for V2X sidelink communication. | - |
| ***v2x-HighPower***Indicates whether the UE supports maximum transmit power associated with Power class 2 V2X UE for V2X sidelink transmission in a band, see TS 36.101 [42]. | - |
| ***v2x-HighReception***Indicates whether the UE supports reception of 20 PSCCH in a subframe and decoding of 136 RBs per subframe counting both PSCCH and PSSCH in a band for V2X sidelink communication. | - |
| ***v2x-nonAdjacentPSCCH-PSSCH***Indicates whether the UE supports transmission and reception in the configuration of non-adjacent PSCCH and PSSCH for V2X sidelink communication. | - |
| ***v2x-numberTxRxTiming***Indicates the number of multiple reference TX/RX timings counted over all the configured sidelink carriers for V2X sidelink communication. | - |
| ***v2x-SensingReportingMode3***Indicates whether the UE supports sensing measurements and reporting of measurement results in eNB scheduled mode for V2X sidelink communication. | - |
| ***v2x-SupportedBandCombinationList***Indicates the supported band combination list on which the UE supports simultaneous transmission and/or reception of V2X sidelink communication. |  |
| ***v2x-SupportedBandCombinationListEUTRA-NR***Indicates the supported band combination list on which the UE supports simultaneous transmission and/or reception of NR sidelink communication only, or joint V2X sidelink communication and NR sidelink communication.  | - |
| ***v2x-SupportedTxBandCombListPerBC, v2x-SupportedRxBandCombListPerBC***Indicates, for a particular band combination of EUTRA, the supported band combination list among *v2x-SupportedBandCombinationList* on which the UE supports simultaneous transmission or reception of EUTRA and V2X sidelink communication respectively. The first bit refers to the first entry of *v2x-SupportedBandCombinationList*, with value 1 indicating V2X sidelink transmission/reception is supported. | - |
| ***v2x-SupportedTxBandCombListPerBC-v1630, v2x-SupportedRxBandCombListPerBC-v1630***Indicates, for a particular band combination of EUTRA, the supported band combination list among *v2x-SupportedBandCombinationListEUTRA-NR* on which the UE supports simultaneous transmission or reception of EUTRA and NR sidelink communication respectively, or simultaneous transmission or reception of EUTRA and joint V2X sidelink communication and NR sidelink communication respectively. The first bit refers to the first entry of *v2x-SupportedBandCombinationListEUTRA-NR*, with value 1 indicating V2X sidelink transmission/reception is supported. | - |
| ***v2x-TxWithShortResvInterval***Indicates whether the UE supports 20 ms and 50 ms resource reservation periods for UE autonomous resource selection and eNB scheduled resource allocation for V2X sidelink communication. | - |
| ***virtualCellID-BasicSRS***Indicates whether the UE supports virtual cell ID for basic SRS symbol(s). | - |
| ***virtualCellID-AddSRS***This field indicates whether the UE supports virtual cell ID for additional SRS symbol(s). | - |
| ***voiceOverPS-HS-UTRA-FDD***Indicates whether UE supports IMS voice according to GSMA IR.58 profile in UTRA FDD. | - |
| ***voiceOverPS-HS-UTRA-TDD128***Indicates whether UE supports IMS voice in UTRA TDD 1.28Mcps. | - |
| ***widebandPRG-Slot, widebandPRG-Subslot, widebandPRG-Subframe***Indicates whether the UE supports wideband precoding resource block group size for slot/subslot/subframe operation as specified in TS 36.213 [23]. | - |
| ***wlan-IW-RAN-Rules***Indicates whether the UE supports RAN-assisted WLAN interworking based on access network selection and traffic steering rules. | - |
| ***wlan-IW-ANDSF-Policies***Indicates whether the UE supports RAN-assisted WLAN interworking based on ANDSF policies. | - |
| ***wlan-MAC-Address***Indicates the WLAN MAC address of this UE. | - |
| ***wlan-PeriodicMeas***Indicates whether the UE supports periodic reporting of WLAN measurements. | - |
| ***wlan-ReportAnyWLAN***Indicates whether the UE supports reporting of WLANs not listed in the *measObjectWLAN*. | - |
| ***wlan-SupportedDataRate***Indicates the maximum WLAN data rate supported by the UE over all LWA bearers. Actual value of supported data rate is field value \* 10 Mbps (i.e., value 1 corresponds to 10 Mbps, value 2 corresponds to 20 Mbps and so on).  | - |
| ***zp-CSI-RS-AperiodicInfo***Indicates whether the UE supports aperiodic ZP-CSI-RS transmission for the indicated transmission mode. | Yes |

NOTE 1: The IE *UE-EUTRA-Capability* does not include AS security capability information, since these are the same as the security capabilities that are signalled by NAS. Consequently, AS need not provide "man-in-the-middle" protection for the security capabilities.

NOTE 2: The column FDD/ TDD diff indicates if the UE is allowed to signal, as part of the additional capabilities for an XDD mode i.e. within *UE-EUTRA-CapabilityAddXDD-Mode-xNM*, a different value compared to the value signalled elsewhere within *UE-EUTRA-Capability* (i.e. the common value, supported for both XDD modes). A '-' is used to indicate that it is not possible to signal different values (used for fields for which the field description is provided for other reasons). Annex E specifies for which TDD and FDD serving cells a UE supporting TDD/FDD CA shall support a capability for which it indicates support within the capability signalling.

NOTE 2a: From REL-15 onwards, the UE is not allowed to signal different values for FDD and TDD unless yes is indicated in column FDD/ TDD diff (i.e. no need to introduce field description solely for the purpose of indicate no).

NOTE 3: The *BandCombinationParameters* for the same band combination can be included more than once.

NOTE 4: UE CA and measurement capabilities indicate the combinations of frequencies that can be configured as serving frequencies.

NOTE 5: The grouping of the cells to the first and second cell group, as indicated by *supportedCellGrouping*, is shown in the table below. The leading / leftmost bit of *supportedCellGrouping* corresponds to the Bit String Position 1.

|  |  |  |  |
| --- | --- | --- | --- |
| Nr of Band Entries: | 5 | 4 | 3 |
| Length of Bit-String: | 15 | 7 | 3 |
| Bit String Position | Cell grouping option (0= first cell group, 1= second cell group) |
| 1 | 00001 | 0001 | 001 |
| 2 | 00010 | 0010 | 010 |
| 3 | 00011 | 0011 | 011 |
| 4 | 00100 | 0100 |  |
| 5 | 00101 | 0101 |  |
| 6 | 00110 | 0110 |  |
| 7 | 00111 | 0111 |  |
| 8 | 01000 |  |  |
| 9 | 01001 |  |  |
| 10 | 01010 |  |  |
| 11 | 01011 |  |  |
| 12 | 01100 |  |  |
| 13 | 01101 |  |  |
| 14 | 01110 |  |  |
| 15 | 01111 |  |  |

NOTE 6: UE includes the *intraBandContiguousCC-InfoList-r12* also for bandwidth class A because of the presence conditions in *BandCombinationParameters-v1270*. For example, if UE supports CA\_1A\_41D band combination, if UE includes the field *intraBandContiguousCC-InfoList-r12* for band 41, the UE includes *intraBandContiguousCC-InfoList-r12* also for band 1.

NOTE 6a: For multiple *BandParameters* entries with the same *bandEUTRA* and same *ca-BandwidthClassDL* in a supported band combination, the UE capabilities indicated by *BandParameters* are agnostic to the order in which they are indicated in the *bandParameterList*, under the condition that the set of the capabilities indicated for the concerned *bandEUTRA* (e.g. *bandParametersDL* and *bandParametersUL)* are used together, and the concerned *BandParameters* correspond to the *supportedBandwithCombinationSet* for which set of channel bandwidths for carrier(s) is the same among sub-blocks, as defined in TS 36.101 [42], Table 5.6A.1-3, Table 5.6A.1-4, Table 5.6A.1-5.

NOTE 7: For a UE that indicates release X in field *accessStratumRelease* but supports a feature specified in release X+ N (i.e. early UE implementation), the ASN.1 comprehension requirement are specified in Annex F.

NOTE 8: For a UE that does not include *mimo-WeightedLayersCapabilities-r13*, or for the case with no CC configured with FD-MIMO, the FD-MIMO processing capability condition is not applicable (i.e. considered as satisfied). For a UE that includes *mimo-WeightedLayersCapabilities-r13*, the FD-MIMO processing capability condition is satisfied if the equation 4.3.28.13-1 in TS 36.306 [5] is satisfied.

<Irrelevant Texts Omitted>

|  |
| --- |
| Next change |

## 6.4 RRC multiplicity and type constraint values

### – Multiplicity and type constraint definitions

-- ASN1START

maxAccessCat-1-r15 INTEGER ::= 63 -- Maximum number of Access Categories - 1

maxACDC-Cat-r13 INTEGER ::= 16 -- Maximum number of ACDC categories (per PLMN)

maxAvailNarrowBands-r13 INTEGER ::= 16 -- Maximum number of narrowbands

maxAvailNarrowBands-1-r16 INTEGER ::= 15 -- Maximum number of narrowbands minus one

maxBandComb-r10 INTEGER ::= 128 -- Maximum number of band combinations.

maxBandComb-r11 INTEGER ::= 256 -- Maximum number of additional band combinations.

maxBandComb-r13 INTEGER ::= 384 -- Maximum number of band combinations in Rel-13

maxBandCombSidelinkNR-r16 INTEGER ::= 512 -- Maximum number of NR sidelink band combinations

maxBands INTEGER ::= 64 -- Maximum number of bands listed in EUTRA UE caps

maxBandsNR-r15 INTEGER ::= 1024 -- Maximum number of NR bands listed in EUTRA UE caps

maxBandsENDC-r16 INTEGER ::= 10 -- Maximum number of NR bands from across all the PLMNs

 -- sharing the serving cell in EN-DC for the forwarding

 -- of *upperLayerIndication*.

maxBandwidthClass-r10 INTEGER ::= 16 -- Maximum number of supported CA BW classes per band

maxBandwidthCombSet-r10 INTEGER ::= 32 -- Maximum number of bandwidth combination sets per

 -- supported band combination

maxBarringInfoSet-r15 INTEGER ::= 8 -- Maximum number of UAC barring information sets

maxBT-IdReport-r15 INTEGER ::= 32 -- Maximum number of Bluetooth IDs to report

maxBT-Name-r15 INTEGER ::= 4 -- Maximum number of Bluetooth name

maxCBR-Level-r14 INTEGER ::= 16 -- Maximum number of CBR levels

maxCBR-Level-1-r14 INTEGER ::= 15

maxCBR-Report-r14 INTEGER ::= 72 -- Maximum number of CBR results in a report

maxCDMA-BandClass INTEGER ::= 32 -- Maximum value of the CDMA band classes

maxCE-Level-r13 INTEGER ::= 4 -- Maximum number of CE levels

maxExcludedCell INTEGER ::= 16 -- Maximum number of exclude-listed physical cell identity

 -- ranges listed in SIB type 4 and 5

maxCellHistory-r12 INTEGER ::= 16 -- Maximum number of visited EUTRA cells reported

maxCellInfoGERAN-r9 INTEGER ::= 32 -- Maximum number of GERAN cells for which system in-

 -- formation can be provided as redirection assistance

maxCellInfoUTRA-r9 INTEGER ::= 16 -- Maximum number of UTRA cells for which system

 -- information can be provided as redirection

 -- assistance

maxCellMeasIdle-r15 INTEGER ::= 8 -- Maximum number of neighbouring inter-frequency

 -- cells per carrier measured in RRC\_IDLE and RRC\_INACTIVE

maxCellNR-r17 INTEGER ::= 8 -- Maximum number of NR cells

maxCombIDC-r11 INTEGER ::= 128 -- Maximum number of reported UL CA or

 -- MR-DC combinations

maxCSI-IM-r11 INTEGER ::= 3 -- Maximum number of CSI-IM configurations

 -- (per carrier frequency)

maxCSI-IM-r12 INTEGER ::= 4 -- Maximum number of CSI-IM configurations

 -- (per carrier frequency)

minCSI-IM-r13 INTEGER ::= 5 -- Minimum number of CSI IM configurations from which

 -- REL-13 extension is used

maxCSI-IM-r13 INTEGER ::= 24 -- Maximum number of CSI-IM configurations

 -- (per carrier frequency)

maxCSI-IM-v1310 INTEGER ::= 20 -- Maximum number of additional CSI-IM configurations

 -- (per carrier frequency)

maxCSI-Proc-r11 INTEGER ::= 4 -- Maximum number of CSI processes (per carrier

 -- frequency)

maxCSI-RS-NZP-r11 INTEGER ::= 3 -- Maximum number of CSI RS resource

 -- configurations using non-zero Tx power

 -- (per carrier frequency)

minCSI-RS-NZP-r13 INTEGER ::= 4 -- Minimum number of CSI RS resource from which

 -- REL-13 extension is used

maxCSI-RS-NZP-r13 INTEGER ::= 24 -- Maximum number of CSI RS resource

 -- configurations using non-zero Tx power

 -- (per carrier frequency)

maxCSI-RS-NZP-v1310 INTEGER ::= 21 -- Maximum number of additional CSI RS resource

 -- configurations using non-zero Tx power

 -- (per carrier frequency)

maxCSI-RS-ZP-r11 INTEGER ::= 4 -- Maximum number of CSI RS resource

 -- configurations using zero Tx power(per carrier

 -- frequency)

maxCQI-ProcExt-r11 INTEGER ::= 3 -- Maximum number of additional periodic CQI

 -- configurations (per carrier frequency)

maxFreqUTRA-TDD-r10 INTEGER ::= 6 -- Maximum number of UTRA TDD carrier frequencies for

 -- which system information can be provided as

 -- redirection assistance

maxCellInter INTEGER ::= 16 -- Maximum number of neighbouring inter-frequency

 -- cells listed in SIB type 5

maxCellIntra INTEGER ::= 16 -- Maximum number of neighbouring intra-frequency

 -- cells listed in SIB type 4

maxCellListGERAN INTEGER ::= 3 -- Maximum number of lists of GERAN cells

maxCellMeas INTEGER ::= 32 -- Maximum number of entries in each of the

 -- cell lists in a measurement object

maxCellRAReportNR-r18 INTEGER ::= 8 -- Maximum number of unique Cells identities of RA

 -- reports included in the NR RA report container

maxCellReport INTEGER ::= 8 -- Maximum number of reported cells/CSI-RS resources

maxCellSFTD INTEGER ::= 3 -- Maximum number of cells for SFTD reporting

maxCellAllowedNR-r16 INTEGER ::= 16 -- Maximum number of allowlisted NR cells in SIB24

maxCondConfig-r16 INTEGER ::= 8 -- Maximum number of conditional configurations

maxConfigSPS-r14 INTEGER ::= 8 -- Maximum number of simultaneous SPS configurations

maxConfigSPS-r15 INTEGER ::= 6 -- Maximum number of simultaneous SPS configurations

 -- configured with SPS C-RNTI

maxCSI-RS-Meas-r12 INTEGER ::= 96 -- Maximum number of entries in the CSI-RS list

 -- in a measurement object

maxDRB INTEGER ::= 11 -- Maximum number of Data Radio Bearers

maxDRBExt-r15 INTEGER ::= 4 -- Maximum number of additional DRBs

maxDRB-r15 INTEGER ::= 15 -- Highest value of extended maximum number of DRBs

maxDS-Duration-r12 INTEGER ::= 5 -- Maximum number of subframes in a discovery signals

 -- occasion

maxDS-ZTP-CSI-RS-r12 INTEGER ::= 5 -- Maximum number of zero transmission power CSI-RS for

 -- a serving cell concerning discovery signals

maxEARFCN INTEGER ::= 65535 -- Maximum value of EUTRA carrier frequency

maxEARFCN-Plus1 INTEGER ::= 65536 -- Lowest value extended EARFCN range

maxEARFCN2 INTEGER ::= 262143 -- Highest value extended EARFCN range

maxEPDCCH-Set-r11 INTEGER ::= 2 -- Maximum number of EPDCCH sets

maxFBI INTEGER ::= 64 -- Maximum value of fequency band indicator

maxFBI-NR-r15 INTEGER ::= 1024 -- Highest value FBI range for NR.

maxFBI-Plus1 INTEGER ::= 65 -- Lowest value extended FBI range

maxFBI2 INTEGER ::= 256 -- Highest value extended FBI range

maxFeatureSets-r15 INTEGER ::= 256 -- Total number of feature sets (size of pool)

maxPerCC-FeatureSets-r15 INTEGER ::= 32 -- Total number of CC-specific feature sets

 -- (size of the pool)

maxFreq INTEGER ::= 8 -- Maximum number of carrier frequencies

maxFreq-1-r16 INTEGER ::= 7 -- Maximum number of carrier frequencies

maxFreqIDC-r11 INTEGER ::= 32 -- Maximum number of carrier frequencies that are

 -- affected by the IDC problems

maxFreqIdle-r15 INTEGER ::= 8 -- Maximum number of carrier frequencies for

 -- IDLE mode measurements configured by eNB

maxFreqMBMS-r11 INTEGER ::= 5 -- Maximum number of carrier frequencies for which an

 -- MBMS capable UE may indicate an interest

maxFreqNBIOT-r16 INTEGER ::= 8 -- Maximum number of NB-IoT carrier frequencies that can

 -- be provided as assistance information for inter-RAT

 -- cell selection

maxFreqNR-r15 INTEGER ::= 5 -- Maximum number of NR carrier frequencies for

 -- which a UE may provide measurement results upon

 -- NR SCG failure

maxFreqSL-NR-r16 INTEGER ::= 8 -- Maximum number of NR anchor carrier frequencies on

 -- which configurations for V2X sidelink communication

 -- are provided

maxFreqV2X-r14 INTEGER ::= 8 -- Maximum number of carrier frequencies for which V2X

 -- sidelink communication can be configured

maxFreqV2X-1-r14 INTEGER ::= 7 -- Highest index of frequencies

maxGERAN-SI INTEGER ::= 10 -- Maximum number of GERAN SI blocks that can be

 -- provided as part of NACC information

maxGNFG INTEGER ::= 16 -- Maximum number of GERAN neighbour freq groups

maxGWUS-Groups-1-r16 INTEGER ::= 31 -- Maximum number of groups minus one for each

 -- probability group

maxGWUS-Resources-r16 INTEGER ::= 4 -- Maximum number of GWUS resources for each group

maxGWUS-ProbThresholds-r16 INTEGER ::= 3 -- Maximum number of paging probability thresholds

maxIdleMeasCarriers-r15 INTEGER ::= 3 -- Maximum number of neighbouring inter-

 -- frequency carriers measured in RRC\_IDLE and RRC\_INACTIVE

maxIdleMeasCarriersExt-r16 INTEGER ::= 5 --Additional number of neighbouring inter-

 -- frequency carriers measured in RRC\_IDLE and RRC\_INACTIVE

maxIdleMeasCarriers-r16 INTEGER ::= 8 -- Maximum number of neighbouring inter-

 -- frequency/inter-RAT carriers measured in RRC\_IDLE and RRC\_INACTIVE

maxLCG-r13 INTEGER ::= 4 -- Maximum number of logical channel groups

maxLogMeasReport-r10 INTEGER ::= 520 -- Maximum number of logged measurement entries

 -- that can be reported by the UE in one message

maxLowerMSD-r18 INTEGER ::= 256 -- Maximum number of lower MSD capability sets for

 -- a victim band

maxLowerMSD-Info-r18 INTEGER ::= 64 -- Maximum number of lower MSD capability sets for

 -- a band combination

maxMBSFN-Allocations INTEGER ::= 8 -- Maximum number of MBSFN frame allocations with

 -- different offset

maxMBSFN-Area INTEGER ::= 8

maxMBSFN-Area-1 INTEGER ::= 7

maxMBMS-ServiceListPerUE-r13 INTEGER ::= 15 -- Maximum number of services which the UE can

 -- include in the MBMS interest indication

maxMeasId INTEGER ::= 32

maxMeasId-Plus1 INTEGER ::= 33

maxMeasId-r12 INTEGER ::= 64

maxMultiBands INTEGER ::= 8 -- Maximum number of additional frequency bands

 -- that a cell belongs to

maxMultiBandsNR-r15 INTEGER ::= 32 -- Maximum number of additional NR frequency bands

 -- that a cell belongs to

maxMultiBandsNR-1-r15 INTEGER ::= 31

maxNS-Pmax-r10 INTEGER ::= 8 -- Maximum number of NS and P-Max values per band

maxNAICS-Entries-r12 INTEGER ::= 8 -- Maximum number of supported NAICS combination(s)

maxNeighCell-r12 INTEGER ::= 8 -- Maximum number of neighbouring cells in NAICS

 -- configuration (per carrier frequency)

maxNeighCell-SCPTM-r13 INTEGER ::= 8 -- Maximum number of SCPTM neighbour cells

maxNrofPCI-PerSMTC-r16 INTEGER ::= 64 -- Maximum number of PCIs per SMTC

maxNrofS-NSSAI-r15 INTEGER ::= 8 -- Maximum number of S-NSSAI

maxObjectId INTEGER ::= 32

maxObjectId-Plus1-r13 INTEGER ::= 33

maxObjectId-r13 INTEGER ::= 64

maxP-a-PerNeighCell-r12 INTEGER ::= 3 -- Maximum number of power offsets for a neighbour cell

 -- in NAICS configuration

maxPageRec INTEGER ::= 16 --

maxPhysCellIdRange-r9 INTEGER ::= 4 -- Maximum number of physical cell identity ranges

maxPLMN-r11 INTEGER ::= 6 -- Maximum number of PLMNs

maxPLMN-1-r14 INTEGER ::= 5 -- Maximum number of PLMNs minus one

maxPLMN-r15 INTEGER ::= 8 -- Maximum number of PLMNs for RNA configuration

maxPLMN-NR-r15 INTEGER ::= 12 -- Maximum number of NR PLMNs

maxPNOffset INTEGER ::= 511 -- Maximum number of CDMA2000 PNOffsets

maxPMCH-PerMBSFN INTEGER ::= 15

maxPSSCH-TxConfig-r14 INTEGER ::= 16 -- Maximum number of PSSCH TX configurations

maxQuantSetsNR-r15 INTEGER ::= 2 -- Maximum number of NR quantity configuration sets

maxQCI-r13 INTEGER ::= 6 -- Maximum number of QCIs

maxRAT-Capabilities INTEGER ::= 8 -- Maximum number of interworking RATs (incl EUTRA)

maxRE-MapQCL-r11 INTEGER ::= 4 -- Maximum number of PDSCH RE Mapping configurations

 -- (per carrier frequency)

maxReportConfigId INTEGER ::= 32

maxReservationPeriod-r14 INTEGER ::= 16 -- Maximum number of resource reservation periodicities

 -- for sidelink V2X communication

maxRS-Index-r15 INTEGER ::= 64 -- Maximum number of RS indices

maxRS-Index-1-r15 INTEGER ::= 63 -- Highest value of RS index as used to identify

 -- RS index in RRM reports.

maxRS-IndexCellQual-r15 INTEGER ::= 16 -- Maximum number of RS indices averaged to derive

 -- cell quality for RRM.

maxRS-IndexReport-r15 INTEGER ::= 32 -- Maximum number of RS indices for RRM.

maxRSTD-Freq-r10 INTEGER ::= 3 -- Maximum number of frequency layers for RSTD

 -- measurement

maxSAI-MBMS-r11 INTEGER ::= 64 -- Maximum number of MBMS service area identities

 -- broadcast per carrier frequency

maxSat-r17 INTEGER ::= 4 -- Maximum number of satellites for E-UTRA or NR

maxSCell-r10 INTEGER ::= 4 -- Maximum number of SCells

maxSCell-r13 INTEGER ::= 31 -- Highest value of extended number range of SCells

maxSCellGroups-r15 INTEGER ::= 4 -- Maximum number of SCell common parameter groups

maxSC-MTCH-r13 INTEGER ::= 1023 -- Maximum number of SC-MTCHs in one cell

maxSC-MTCH-BR-r14 INTEGER ::= 128 -- Maximum number of SC-MTCHs in one cell for feMTC

maxSL-CommRxPoolNFreq-r13 INTEGER ::= 32 -- Maximum number of individual sidelink communication

 -- Rx resource pools on neighbouring freq

maxSL-CommRxPoolPreconf-v1310 INTEGER ::= 12 -- Maximum number of additional preconfigured

 -- sidelink communication Rx resource pool entries

maxSL-TxPool-r12Plus1-r13 INTEGER ::= 5 -- First additional individual sidelink

 -- Tx resource pool

maxSL-TxPool-v1310 INTEGER ::= 4 -- Maximum number of additional sidelink

 -- Tx resource pool entries

maxSL-TxPool-r13 INTEGER ::= 8 -- Maximum number of individual sidelink

 -- Tx resource pools

maxSL-CommTxPoolPreconf-v1310 INTEGER ::= 7 -- Maximum number of additional preconfigured

 -- sidelink Tx resource pool entries

maxSL-Dest-r12 INTEGER ::= 16 -- Maximum number of sidelink destinations

maxSL-DiscCells-r13 INTEGER ::= 16 -- Maximum number of cells with similar sidelink

 -- configurations

maxSL-DiscPowerClass-r12 INTEGER ::= 3 -- Maximum number of sidelink power classes

maxSL-DiscRxPoolPreconf-r13 INTEGER ::= 16 -- Maximum number of preconfigured sidelink

 -- discovery Rx resource pool entries

maxSL-DiscSysInfoReportFreq-r13 INTEGER ::= 8 -- Maximum number of frequencies to include in a

 -- SidelinkUEInformation for SI reporting

maxSL-DiscTxPoolPreconf-r13 INTEGER ::= 4 -- Maximum number of preconfigured sidelink

 -- discovery Tx resource pool entries

maxSL-GP-r13 INTEGER ::= 8 -- Maximum number of gap patterns that can be requested

 -- for a frequency or assigned

maxSL-PoolToMeasure-r14 INTEGER ::= 72 -- Maximum number of TX resource pools for CBR

 -- measurement and report

maxSL-Prio-r13 INTEGER ::= 8 -- Maximum number of entries in sidelink priority list

maxSL-RxPool-r12 INTEGER ::= 16 -- Maximum number of individual sidelink Rx resource pools

maxSL-Reliability-r15 INTEGER ::= 8 -- Maximum number of entries in sidelink reliability list

maxSL-SyncConfig-r12 INTEGER ::= 16 -- Maximum number of sidelink Sync configurations

maxSL-TF-IndexPair-r12 INTEGER ::= 64 -- Maximum number of sidelink Time Freq resource index

 -- pairs

maxSL-TxPool-r12 INTEGER ::= 4 -- Maximum number of individual sidelink Tx resource pools

maxSL-V2X-RxPool-r14 INTEGER ::= 16 -- Maximum number of RX resource pools for

 -- V2X sidelink communication

maxSL-V2X-RxPoolPreconf-r14 INTEGER ::= 16 -- Maximum number of RX resource pools for

 -- V2X sidelink communication

maxSL-V2X-TxPool-r14 INTEGER ::= 8 -- Maximum number of TX resource pools for

 -- V2X sidelink communication

maxSL-V2X-TxPoolPreconf-r14 INTEGER ::= 8 -- Maximum number of TX resource pools for

 -- V2X sidelink communication

maxSL-V2X-SyncConfig-r14 INTEGER ::= 16 -- Maximum number of sidelink Sync configurations

 -- for V2X sidelink communication

maxSL-V2X-CBRConfig-r14 INTEGER ::= 4 -- Maximum number of CBR range configurations

 -- for V2X sidelink communication congestion

 -- control

maxSL-V2X-CBRConfig-1-r14 INTEGER ::= 3

maxSL-V2X-TxConfig-r14 INTEGER ::= 64 -- Maximum number of TX parameter configurations

 -- for V2X sidelink communication congestion

 -- control

maxSL-V2X-TxConfig-1-r14 INTEGER ::= 63

maxSL-V2X-CBRConfig2-r14 INTEGER ::= 8 -- Maximum number of CBR range configurations in

 -- pre-configuration for V2X sidelink

 -- communication congestion control

maxSL-V2X-CBRConfig2-1-r14 INTEGER ::= 7

maxSL-V2X-TxConfig2-r14 INTEGER ::= 128 -- Maximum number of TX parameter

 -- configurations in pre-configuration for V2X

 -- sidelink communication congestion control

maxSL-V2X-TxConfig2-1-r14 INTEGER ::= 127

maxSTAG-r11 INTEGER ::= 3 -- Maximum number of STAGs

maxServCell-r10 INTEGER ::= 5 -- Maximum number of Serving cells

maxServCell-r13 INTEGER ::= 32 -- Highest value of extended number range of Serving cells

maxServCellNR-r15 INTEGER ::= 16 -- Maximum number of NR serving cells

maxServiceCount INTEGER ::= 16 -- Maximum number of MBMS services that can be included

 -- in an MBMS counting request and response

maxServiceCount-1 INTEGER ::= 15

maxSessionPerPMCH INTEGER ::= 29

maxSessionPerPMCH-1 INTEGER ::= 28

maxSIB INTEGER ::= 32 -- Maximum number of SIBs

maxSIB-1 INTEGER ::= 31

maxSI-Message INTEGER ::= 32 -- Maximum number of SI messages

maxSimultaneousBands-r10 INTEGER ::= 64 -- Maximum number of simultaneously aggregated bands

maxSubframePatternIDC-r11 INTEGER ::= 8 -- Maximum number of subframe reservation patterns

 -- that the UE can simultaneously recommend to the

 -- E-UTRAN for use.

maxTAC-r17 INTEGER ::= 12 -- Maximum number of Tracking Area Codes

 -- broadcast in a cell

maxTrafficPattern-r14 INTEGER ::= 8 -- Maximum number of periodical traffic patterns

 -- that the UE can simultaneously report to the

 -- E-UTRAN.

maxUTRA-FDD-Carrier INTEGER ::= 16 -- Maximum number of UTRA FDD carrier frequencies

maxUTRA-TDD-Carrier INTEGER ::= 16 -- Maximum number of UTRA TDD carrier frequencies

maxWayPoint-r15 INTEGER ::= 20 -- Maximum number of flight path information waypoints

maxWLAN-Id-r12 INTEGER ::= 16 -- Maximum number of WLAN identifiers

maxWLAN-Bands-r13 INTEGER ::= 8 -- Maximum number of WLAN bands

maxWLAN-Id-r13 INTEGER ::= 32 -- Maximum number of WLAN identifiers

maxWLAN-Channels-r13 INTEGER ::= 16 -- maximum number of WLAN channels used in

-- WLAN-CarrierInfo

maxWLAN-CarrierInfo-r13 INTEGER ::= 8 -- Maximum number of WLAN Carrier Information

maxWLAN-Id-Report-r14 INTEGER ::= 32 -- Maximum number of WLAN IDs to report

maxWLAN-Name-r15 INTEGER ::= 4 -- Maximum number of WLAN name

-- ASN1STOP

NOTE: The value of maxDRB aligns with SA2.

### – End of EUTRA-RRC-Definitions

-- ASN1START

END

-- ASN1STOP

|  |
| --- |
| End of change |