**3GPP TSG-RAN WG2 Meeting #131** **R2-250xxxx
Bengaluru, India, August 25-29, 2025**

**Agenda item: 8.5.1**

**Source: InterDigital (Rapporteur)**

**Title: [POST130][109][NES] 38.321 CR (InterDigital)**

**Document for: Discussion and Decision**

# Introduction

This document collects the comments received during the following email discussion on the MAC CR for the R19 NES work item:

**[POST130][109][NES] (IDC)**

 **Scope:** Update 38.321 running CR (also including this meeting’s agreements and latest other RAN WGs’ inputs) and remaining essential MAC open issues.

 **Intended outcome:** 38.321 running CR and remaining essential MAC open issues.

**Deadline:** Long email discussion.

## Contact information:

|  |  |  |
| --- | --- | --- |
| Company | Delegate Name | Email |
| OPPO | Qianxi Lu | qianxi.lu@oppo.com |
| Sharp | LIU Lei | lei.liu@cn.sharp-world.com |
| Fujitsu | Katsunari Uemura | u-katsunari@fujitsu.com |
| Xiaomi | Li Zhao | Zhaoli6@xiaomi.com |
| Apple | Peng Cheng | pcheng24@apple.com |
| Ericsson | Helka-Liina Määttänen | Helka-liina.maattanen@ericsson.com |

# Discussion on TS 38.321 running CR

Companies can provide comments and suggestions to the uploaded running CR in this table. Please do not add changes, suggestions, or comments directly to the draft CR document.

|  |  |  |
| --- | --- | --- |
| Company + Issue Number (e.g., ID001) | Issue | Comments and proposed changes |
| OPPO001 | NOTE 5: if CB-PreamblesPerSSB is configured for additional ROs in addl-RACH-Config-Adaptation , UE selects only amongst preambles configured for the next valid RO(s) associated with the selected SSB. | [OPPO] The yellow part may lead to question on whether there is a case where CB-PreamblesPerSSB is NOT configured. Suggested change is to simplify the text to like ‘if addl-RACH-Config-Adaptation is configured’.[Rapp]: Looking at the RRC running CR, it seems like the parameter “ssb-perRACH-OccasionAndCB-PreamblesPerSSB-r19” is optional under “RandomAccessAdaptationConfig-r19”The note is updated in v2 according to the comments under Samsung001 |
| OPPO002 | It has a variable size; it includes an Activation/Deactivation bitmap and, in ascending order based on the ServCellIndex ,Ci: If there is an SCell configured for the MAC entity with *SCellIndex i* as specified in TS 38.331 [5], this field indicates the on-demand SSB activation/deactivation status for the SCell with *SCellIndex* i | [OPPO] To unify the ordering reference to SCellIndex.[Rapp]: “*SCellIndex*” is used in v2 for both instances. |
| Samsung 001 | NOTE 5: if CB-PreamblesPerSSB is configured for additional ROs in addl-RACH-Config-Adaptation , UE selects only amongst preambles configured for the next valid RO(s) associated with the selected SSB.Note seems not correct. Our understanding is that:UE may select RO corresponding to selected SSB from a) additional ROs or b) legacy ROsFor a)* if ssb-perRACH-OccasionAndCB-PreamblesPerSSB is configured in addl-RACH-Config-Adaptation, UE selects preamble corresponding to selected SSB amongst the preambles determined based on ssb-perRACH-OccasionAndCB-PreamblesPerSSB in addl-RACH-Config-Adaptation
* if ssb-perRACH-OccasionAndCB-PreamblesPerSSB is not configured in addl-RACH-Config-Adaptation, UE selects preamble corresponding to selected SSB amongst the preambles determined based on ssb-perRACH-OccasionAndCB-PreamblesPerSSB in RACH-ConfigCommon

For b)* UE selects preamble corresponding to selected SSB amongst the preambles determined based on ssb-perRACH-OccasionAndCB-PreamblesPerSSB in RACH-ConfigCommon
 | I think note should be something like:If RO selected for preamble transmission is configured by addl-RACH-Config-Adaptation and ssb-perRACH-OccasionAndCB-PreamblesPerSSB is configured in addl-RACH-Config-Adaptation, UE selects preamble corresponding to selected SSB amongst the preambles determined according to ssb-perRACH-OccasionAndCB-PreamblesPerSSB in addl-RACH-Config-Adaptation. Otherwise, UE selects preamble corresponding to selected SSB amongst the preambles determined according to ssb-perRACH-OccasionAndCB-PreamblesPerSSB in RACH-ConfigCommon.[Rapp]: Thanks for this clarification. Indeed, the intent was to clarify for case a). I have updated the note in v2 according to this suggestion. Companies can comment if the note should not capture this part for legacy ROs selected. The updated note captures both cases now in v2.[vivo] Maybe we only need to clarify the case when the UE selects additional RO. When legacy RO is selected, the procedure is the same as legacy.[Fujitsu] Agree with vivo. As it is the legacy case, the last part is not needed.[Apple] Same view as vivo. It is just a NOTE, and not necessary to include legacy case.[OPPO] OK to refer to the ssb-perRACH-OccasionAndCB-PreamblesPerSSB in RACH-ConfigCommon when not configured for additional RACH. But this seems normally captured in RRC rather than in MAC, as in legacy spec (?) So that we prefer to do it same way, i.e., reflect in 331 specifically which ssb-perRACH-OccasionAndCB-PreamblesPerSSB parameter to use (in addl-RACH-Config-Adaptation if present, or in RACH-ConfigCommon otherwise). While in 321, we can use a simplified wording, like If RO selected for preamble transmission is configured by addl-RACH-Config-Adaptation, UE selects preamble corresponding to selected SSB amongst the preambles determined according to the applicable ssb-perRACH-OccasionAndCB-PreamblesPerSSB [Rapp]: based on further comments above, this part was removed in v3.Regarding whether to capture this in MAC or RRC, the intention here is just to capture this agreement as it is about preamble selection (done in MAC):A note in TS 38.321 is added to clarify that UE selects only amongst preambles configured for the next valid RO(s) for the selected SSB, when CB-PreamblesPerSSB is configured for additional ROs |
| Samsung 002 | The description of cases in which the UE applies the additional ROs are missing. We need some text like:1>if the random access procedure was initiated by SI request or SIB1 request or reconfiguration with sync or LTM cell switch or PDCCH order for LTM candidate cell; or1>if contention free random access preamble is selected for PRACH transmission:1. The PRACH occasions configured by *addl-RACH-Config-Adaptation* in the RACH-ConfigCommon of selected random access resource set is not applied for PRACH transmission.

1>Else:1. The PRACH occasions configured by *addl-RACH-Config-Adaptation* in the RACH-ConfigCommon of selected random access resource set is applicable for PRACH transmission, if available (as specified in TS 38.213/38.212).
 | [Rapp]: I understand you want to explicitly capture these agreements:From R2 perspective, not apply time-domain RACH adaptation to RACH resources for MSG1-based SI request.RACH adaptation is not applied to the following cases (for non-serving cell case): 1) PDCCH order for additional RACH; 2) L3 HO command. 3) LTM CSC MAC-CE; 4) PDCCH order for LTM early UL sync;RACH adaptation is not applied to BFR.I added the following at the bottom of section 5.1.1b in v2:1> if the Random Access procedure was initiated by SI request, SIB1 request, reconfiguration with sync, beam failure recovery, LTM Cell Switch, or PDCCH order for an LTM candidate cell:2> PRACH occasions configured by *addlRACH-Config-Adaptation* in *RACH-ConfigCommon* of the selected set of Random Access resources are not applicable for this Random Access procedure.1> else:2> PRACH occasions configured by *addlRACH-Config-Adaptation* in *RACH-ConfigCommon* of the selected set of Random Access resources are applicable for this Random Access procedure, if available (as specified in TS 38.213 [6] and 38.212 [9]). |
| Samsung 003 |  ConfigIndexi: The on-demand SSB configuration index to apply for *SCellIndex i* as. This field is present for SCell with SCellIndex *i* if Ci is 1, and not present if Ci is 0.Incomplete sentence. Instead of repeating “specified in TS 38.331 [5]”, rather “as” should be dropped. | [Rapp]: adopted in v2. |
| Samsung 004 | Oct 2 should also be marked as optional in figure **6.1.3.x-1** | [Rapp]: adopted in v2. |
| Samsung 005 | Oct 5 should also be marked as optional in figure **6.1.3.x-2** | [Rapp]: adopted in v2. |
| Samsung 005 | Editor’s note: the size of OD-SSB ConfigIndexi is FFSWrong format. Use subscript. | [Rapp]: adopted in v2. |
| Sharp 001 | The On-demand SSB Activation/Deactivation MAC CE of one Activation/Deactivation octet is identified by a MAC subheader with eLCID as specified in Table 6.2.1-1b. It has a variable size; it includes an Activation/Deactivation bitmap and, in ascending order based on the *ServCellIndex*, an on-demand SSB configuration index field for each SCell activated in the bitmap.[Sharp]: The highlighted wording might be misunderstood as for each activated SCell. | Suggested modification: for each SCell on which On-Demand SSB transmission is activated in the bitmap.Or just remove “activated” since the detailed description for the fields below has shown the exact meaning.[Rapp]: adopted in v2. |
| Sharp 002 | 5.1.1 Random Access procedure initialization1> perform the BWP operation as specified in clause 5.15, except when the Random Access procedure is initiated by the PDCCH order for an LTM candidate cell;[Sharp]: Currently, for random access procedure, during BWP operation UE may need to switch UL/DL BWP for a random access procedure. Such BWP operation is not applicable for random access for SIB1 request, since RACH resources for SIB1 request is not associated with UL BWP. | Suggested modification:1> perform the B38te cell or initiated for SIB1 request;[Rapp]: No exception seem to be captured other SI as well. I will let companies comment on this, before writing a conclusion.[Sharp]: This issue is for RRC CONNECTED. BWP operation for random access seems to have no impacts on IDLE/INACTIVE. In RRC CONNECTED, other SI request doesn’t initiate random access, but SIB1 request initiates random access while T311 is running.[Apple] I have some sympathy with Rapp. For CONNECTE UE with T311 running, its RACH behaviour should be same as IDLE/INACTIVE UE because default L1 parameter and MAC cell group configuration is used (section 5.3.7.3 of 38.331)2> apply the default L1 parameter values as specified in corresponding physical layer specifications except for the parameters for which values are provided in *SIB1*;2> apply the default MAC Cell Group configuration as specified in 9.2.2;Thus, my view is that this case can also refer to clause 5.15. [Rapp]: No change pursued for now. It can be reconsidered if more views are expressed. |
| Fujitsu 001 | 5.1.3 Random Access Preamble transmission…1> if LBT failure indication is received from lower layers for this Random Access Preamble transmission:… 5> if this Random Access procedure was triggered for SI request or SIB1 request: | [Fujitsu] In RAN1#121 there is a conclusion as following: **Conclusion**There is no consensus on the support of OD-SIB1 for NR-U in Rel-19.It means that SIB1 request is not triggered for unlicensed cells. So, we would like to suggest removing “or SIB1 request”.[Rapp]: it is removed in v3, following the R1 conclusion. |
| Fujitsu 002 | 6.1.3.x On-demand SSB Activation/Deactivation MAC CE... A single octet bitmap is used for Activation/Deactivation of the On-Demand SSB transmission and indicating the presence of an on-demand SSB configuration index per Serving Cell, containing seven C-fields and one R-field.... A four-octet bitmap is used for Activation/Deactivation of the On-Demand SSB transmission and indicating the presence of an on-demand SSB configuration index per Serving Cell, containing 31 C-fields and one R-field.- ConfigIndexi: The on-demand SSB configuration index to apply for *SCellIndex i*. This field is present for SCell with SCellIndex *i* if Ci is 1, and not present if Ci is 0. | [Fujitsu] OD-SSB is configured only for SCells, For clarification, the yellow highlighted part should be “SCell”.The cyan highlighted part should be *italic*.[Rapp]: adopted in v3. |
| Fujitsu 003 | 6.1.3.x On-demand SSB Activation/Deactivation MAC CE- ConfigIndexi: The on-demand SSB configuration index to apply for *SCellIndex i*. This field is present for SCell with SCellIndex *i* if Ci is 1, and not present if Ci is 0. | [Fujitsu] We understand the index size is FFS, but based on the current figure, if SCell index i is set to 0, the octet containing ConfigIndex i is not included. To clarify that, the text can be updated as follows: - ConfigIndexi: The on-demand SSB configuration index to apply for *SCellIndex i*. The octet containing this field is present for SCell with SCellIndex *i* if Ci is 1, and the octet is not present if Ci is 0.[Rapp]: adopted in v3. |
| Xiaomi001 | A typo. - ConfigIndexi: The on-demand SSB configuration index to apply for *SCellIndex i* ~~as~~. This field is present for SCell with SCellIndex *i* if Ci is 1, and not present if Ci is 0. | [Xiaomi] “as” should be deleted[Rapp]: removed in v2. |
| Apple 001 | 1> if the Random Access procedure was initiated by SI request, SIB1 request, reconfiguration with sync, beam failure recovery, LTM Cell Switch, or PDCCH order for an LTM candidate cell:2> PRACH occasions configured by *addlRACH-Config-Adaptation* in *RACH-ConfigCommon* of the selected set of Random Access resources are not applicable for this Random Access procedure.1> else:2> PRACH occasions configured by *addlRACH-Config-Adaptation* in *RACH-ConfigCommon* of the selected set of Random Access resources are applicable for this Random Access procedure, if available (as specified in TS 38.213 [6] and 38.212 [9]). | [Apple] I think the highlighted case seems not to be aligned with the following agreement (1 is for the case of PDCCH order for two-TA case):* RACH adaptation is not applied to the following cases (for non-serving cell case):

1) PDCCH order for additional RACH;2) L3 HO command.3) LTM CSC MAC-CE;4) PDCCH order for LTM early UL sync;Note that “two-TA RACH” include intra-cell and inter-cell case. My understanding is only for inter-cell case. Thus, maybe we can modify it to “PDCCH order for an ~~LTM candidate cell~~ non-serving cell. [Rapp]: adopted in v3.[ER] Apple is talking about 2TA and that is different feature from LTM. In that context intercell or nonserving cell means an additional PCI within the serving cell(there is only one serving cell even in this so called inter-cell case). Term non-serving cell is also not defined and should be removed.[Rapp]: Changed in v4 to “PDCCH order for an LTM candidate cell" and "PDCCH order with the PRACH association indicator field in DCI set to 1", to avoid ambiguity. |
| Fujitsu 004 | 5.1.4 Random Access Response reception2> else:3> start the *ra-ResponseWindow* configured in *RACH-ConfigCommon* at the first PDCCH occasion as specified in TS 38.213 [6] from the end of the Random Access Preamble transmission.…1> if *ra-ResponseWindow* configured in *RACH-ConfigCommon* expires, and if the Random Access Response containing Random Access Preamble identifiers that matches the transmitted *PREAMBLE\_INDEX* has not been received:2> consider the Random Access Response reception not successful; | [Fujitsu] In the current RRC running CR, the ra-ResponseWindow for receiving the acknowledgement of SIB1 request is configured in *RACHConfig-SIB1* in SIBxx but not in *RACH-ConfigCommon*. To align the MAC spec and RRC spec, the text can be updated as:2> else if the Random Access Preamble is transmitted for SIB1 request:3> start the *ra-ResponseWindow* configured in *RACH-ConfigSIB1* at the first PDCCH occasion as specified in TS 38.213 [6] from the end of the Random Access Preamble transmission.2> else:3> start the *ra-ResponseWindow* configured in *RACH-ConfigCommon* at the first PDCCH occasion as specified in TS 38.213 [6] from the end of the Random Access Preamble transmission.…1> if *ra-ResponseWindow* configured in *RACH-ConfigCommon* or *RACH-ConfigSIB1* expires, and if the Random Access Response containing Random Access Preamble identifiers that matches the transmitted *PREAMBLE\_INDEX* has not been received:2> consider the Random Access Response reception not successful;[Rapp]: adopted in v3. |
| HW001 | On the format of OD-SSB MAC CE, to incorporate the following agreement, we think Cj=1 means that the UE will apply the corresponding configuration index:* For implicit deactivation of an OD-SSB transmission after the transmission of N occasions, reuse to SCell deactivation timer behaviour: UE (re)-applies the indicated N value in the MAC CE for each activated OD-SSB transmission upon reception of the OD-SSB Activation/Deactivation MAC CE.
 | Proposed change:The Ci field is set to 1 to indicate that on-demand SSB transmission on the SCell with *SCellIndex* i shall be activated with the corresponding on-demand SSB configuration index to be applied.[Rapp]: adopted in v3. |
| ER01 | In our view the addition at the bottom of section 5.1.1b in v2, below, is not needed. The selection is already completed at this point, so this should either be captured separately for each case, e.g., LTM Cell Switch, SI request etc., before resource selection or above all (if possible at all using the current framework). Further, a better place for this is just before “*NOTE 1: Void.*”. 1. After the notes, all procedural text is about selection of RA resources.

1> if the Random Access procedure was initiated by SI request, SIB1 request, reconfiguration with sync, beam failure recovery, LTM Cell Switch, or PDCCH order for an LTM candidate cell:2> PRACH occasions configured by *addlRACH-Config-Adaptation* in *RACH-ConfigCommon* of the selected set of Random Access resources are not applicable for this Random Access procedure.1> else:2> PRACH occasions configured by *addlRACH-Config-Adaptation* in *RACH-ConfigCommon* of the selected set of Random Access resources are applicable for this Random Access procedure, if available (as specified in TS 38.213 [6] and 38.212 [9]). | [Rapp]: Moved in v4 to before “NOTE 1: Void.”I have not removed it, as now the deadline has passed, and comments were received to capture those agreements. |
| ER02 | The below note should be numbered as X and there is and which should be non-italic.NOTE 5: If an RO selected for preamble transmission is configured by *addlRACH-Config-Adaptation* *and ssb-perRACH-OccasionAndCB-PreamblesPerSSB* is configured in *addlRACH-Config-Adaptation*, UE selects preamble corresponding to selected SSB amongst the preambles determined according to *ssb-perRACH-OccasionAndCB-PreamblesPerSSB* in *addlRACH-Config-Adaptation*. | [Rapp]: adopted in v4. |
| ER03 | The MAC-CEs could be shortened if two indexes are in one octet.6 Protocol Data Units, formats and parameters6.1.3 MAC Control Elements (CEs)6.1.3.x On-demand SSB Activation/Deactivation MAC CEThe on-demand SSB Activation/Deactivation MAC CE of one Activation/Deactivation octet is identified by a MAC subheader with eLCID as specified in Table 6.2.1-1b. It has a variable size; it includes an Activation/Deactivation bitmap and, in ascending order based on the *SCellIndex*, an on-demand SSB configuration index field for each SCell on which on-demand SSB is activated in the bitmap. A single octet bitmap is used for Activation/Deactivation of the on-demand SSB transmission and indicating the presence of an on-demand SSB configuration index per Serving Cell, containing seven C-fields and one R-field. The on-demand SSB Activation/Deactivation MAC CE of one Activation/Deactivation octet is defined as follows (Figure 6.1.3.x-1).The on-demand SSB Activation/Deactivation MAC CE of four Activation/Deactivation octets is identified by a MAC subheader with eLCID as specified in Table 6.2.1-1b. It has a variable size; it includes an Activation/Deactivation bitmap and, in ascending order based on the *SCellIndex*, an on-demand SSB configuration index field for each SCell on which on-demand SSB is activated in the bitmap. A four-octet bitmap is used for Activation/Deactivation of the pn-demand SSB transmission and indicating the presence of an on-demand SSB configuration index per Serving Cell, containing 31 C-fields and one R-field. The on-demand SSB Activation/Deactivation MAC CE of four Activation/Deactivation octets is defined as follows (Figure 6.1.3.x-2).- Ci: If there is an SCell configured for the MAC entity with *SCellIndex i* as specified in TS 38.331 [5], this field indicates the on-demand SSB activation/deactivation status for the SCell with *SCellIndex* i, else the MAC entity shall ignore the Ci field. The Ci field is set to 1 to indicate that on-demand SSB transmission on the SCell with *SCellIndex* i shall be activated. The Ci field is set to 0 to indicate that on-demand SSB transmission on the SCell with *SCellIndex* i shall be deactivated;- ConfigIndexi: The on-demand SSB configuration index to apply for *SCellIndex i*. This field is present for SCell with SCellIndex *i* if Ci is 1, and not present if Ci is 0.- R: Reserved bit, set to 0.**Figure 6.1.3.x-1: On-demand SSB Activation/Deactivation MAC CE of one Activation/Deactivation octet****Figure 6.1.3.x-2: On-demand SSB Activation/Deactivation MAC CE of four Activation/Deactivation octets** | [Rapp]: Thank you for your comment. I have not changed the structure of the MAC CE, as the deadline has now passed. I hope this can be an acceptable baseline for now. We can discuss further for further size optimization. |
|  |  |  |

# Conclusion

The running CR is updated considering the comments above.

# Annex A: R2 agreements affecting TS 38.321

Change is introduced to support the following objectives:
- On-demand SSB for SCell operation

- On-demand SIB1 for idle/inactive UEs

- Adaptation of common channels/signals

The following color code is used to categorize agreements interms of if/how they have been captured. It will be removed when the CR is finalized.

Fully implemented
Already specified in MAC
Not/partially implemented but additional agreements/FFSs needed before conclusion
Doesn’t impact MAC spec

**RAN2 Agreements**

**On-demand SSB for SCell operation**

**RAN2#127**

RAN2 start the discussion from Scenario 2/2A and wait for RAN1 conclusion on Scenario 3A/3B

RRC based OD-SSB transmission indication is used to indicate at least the initial activation/deactivation state of OD-SSB configuration. FFS on reconfiguration.

New MAC-CE for OD-SSB transmission indication is introduced. We will not change legacy SCell activation/deactivation MAC CE. FFS if we need further optimization for scenario 2A.

Measurement based on OD-SSB in both case 1 and case 2 will be considered. (case 1 and case 2 defined in RAN1).

For Case #1, the UE does not expect to measure SSB when on-demand SSB transmission is deactivated. In other words, the UE expects to measure SSB when on-demand SSB transmission is activated.

RAN2 does not handle the issue raised in R2-2407414 in OD-SSB based measurements.

R2-2407414: Proposal 3: RAN2 WG to discuss the issue of false measurement report triggering due to no SSB transmission when on-demand SSB is deactivated.

* RAN2 does not handle this issue in OD-SSB

RAN2 study how the UE to perform L3 measurement according to OD-SSB L3 RRM configuration.

**RAN2#127bis**

No need to restrict the OD-SSB activation/deactivation state indication in RRC to initial configuration. No special specification effort is required.

Don’t introduce further new MAC CE that combines SCell activation/deactivation and OD-SSB indication for scenario 2A.

NW should be able to send OD-SSB indication for multiple SCells simultaneously by a MAC CE.

**RAN2#129**

RAN2 leave it to RAN4 to conclude whether always-on SSB and/or OD-SSB are measured when both are transmitted in OD-SSB case 2.

**RAN2#129bis**

For explicit activation/deactivation, the OD-SSB MAC-CE includes fixed sized bitmap to indicate whether OD-SSB is activated in each SCell (i.e., similar to legacy SCell A/D MAC-CE).

A/D bit: “1” means activation, “0” means deactivation for explicit deactivation case.

For explicit activation/deactivation, the OD-SSB MAC-CE supports two formats: one format indicates up to 7 SCells and the other format indicates up to 31 SCells.

OD-SSB MAC-CE includes a configuration index for each SCell activating OD-SSB.

RAN2 aims to define single MAC CE format for both explicit and implicit OD-SSB deactivations. Details are FFS.

Working assumption: When A-SSB and OD-SSB have different center frequency, introduce a new servingCellMO in ServingCellConfig to indicate MO of OD-SSB. FFS if we allow multiple OD-SSBs with the different frequencies for a given SCell.

**RAN2#130**

The configuration index is associated with a set of parameters, i.e., od-ssb-Periodicity, od-ssb-PositionsInBurst and od-ssb-nrofBurst.

The OD-SSB MAC CE is a variable size MAC CE. For each activated OD-SSB SCell, an additional field is added to indicate the applicable OD-SSB configuration index. TP in R2-2504280 will be baseline for the running CR. Detailed wordings can be further discussed.

When UE receives MAC CE with Cj bit set to 0 for an SCell for which OD-SSB is currently activated: OD-SSB is deactivated for the jth SCell, irrespective of whether od-ssb-nrofBurst is included or not included in configuration applied for the activated OD-SSB. Running timer/counter for implicit deactivation (if any) for the SCell is stopped.

For implicit deactivation of an OD-SSB transmission after the transmission of N occasions, reuse to SCell deactivation timer behaviour: UE (re)-applies the indicated N value in the MAC CE for each activated OD-SSB transmission upon reception of the OD-SSB Activation/Deactivation MAC CE.

In L3 measurement in OD-SSB case 1, if MAC-CE/RRC based activation / deactivation:
• The UE starts L3 measurement towards the activated OD-SSB based on configured servingCellMO after reception of the activation.
• The UE stops L3 measurements after it determines the OD-SSB is deactivated implicitly or explicitly.

**On-demand SIB1 for idle/inactive UEs**

**RAN2#125bis**

At least RAN2 starts scenario 1a. Other scenarios are not excluded.

* Scenario 1a: Cell A SIB assisted intra-cell WUS. And WUS and SIB1 is sent to/from NES cell. with below potential RAN2 impacts:
	+ Add WUS configuration in SIB of cell A.
	+ Cell reselection from cell A to NES cell, including trigger condition and cell barring changes.
	+ Whether allow camping, paging and SIB update in NES cell.
	+ Cell reselection from NES cell to cell A or normal cell.

Contents of UL WUS

* RAN2 assumes that RACH procedure is reused for UE to request on-demand SIB1.
* UL WUS configuration includes at least below information:
	+ RACH configuration
* A UE needs to know a UL WUS configuration to request SIB1 of which cell.

On-demand SIB1 acquisition procedure

- Existing Msg 1 based on-demand procedure is reused for on-demand SIB1 acquisition procedure. FFS on Msg 3. FFS if / when the UE monitors the OD-SIB1 upon reception of RAR. FFS:T whether introduce specified UE behavior if RACH failure of OD-SIB1 request.

The UE first should acquire valid SIB1 (e.g. via SIB1 request) for camping to NES cell (if the UE knows the cell doesn’t broadcast SIB1 and supports on-demand SIB1).

**RAN2#126**

Study on-demand SIB1 provisioning for NES Cell(s) in versions of Scenario 1a with multiple Cells A and/or NES Cells:

* More than one Cell A may provide configuration for the same NES cell.
* The same Cell A may assist more than one NES Cells.

RRC release message assisted intra-cell WUS can be discussed as option of signaling details in stage 3.

Can use the PCI and frequency of a NES Cell to associate the UL WUS configuration with a NES Cell.

For Message 1 based on-demand SIB1 request, the on-demand SI request configuration that currently included in SIB1 may be used as the design baseline.

Cell A’s SIB can be used to configure on-demand SIB1 related configuration for neighbour NES cells, e.g., via new SIB or the existing SIB.

If the UE chooses the NES cell using legacy intra-F/inter-F cell re-selection procedure (as baseline), the UE triggers WUS transmission.

After UE successfully receives OD-SIB1 for that NES Cell and if it is a suitable cell, UE camps in the NES Cell “similar” to a legacy Cell.

RAN2 not to support on-demand SIB1 request that is combined with an initial access to perform RRC connection establishment/resume on the NES cell.

NW need to bar the legacy UE from accessing the on-demand SIB1 cell (e.g. based on the existing barring mechanism).

How to avoid/deprioritize the legacy UE camping at the Cell A attempting to switch to the NES Cell (but allowing the R19 NES UE to do that).

If the NES UE is unable to acquire the SIB1 of NES Cell before UE initiates OD-SIB1 procedure, it will not consider it as barred at that moment. R19 NES UE bars the cell if the UE fails to acquire SIB1 via on-demand SIB1 for NES cell.

After Rel-19 NES UEs camp in NES cell, the UE behaviour is same as the one defined as legacy normal camped state, e.g. paging reception, SIB1 update, etc.

RAN2 assumes the UE is expected to receive the RAR responding to the preamble transmission for Msg1-based on-demand SIB1 procedure, as the baseline.

As baseline, upon random access procedure failure of OD-SIB1 request, UE regards OD-SIB1 can’t be acquired in the NES cell and considers it as barred. It doesn’t exclude the option to leave the determination to the UE implementation.

Once the NES UE camps on the NES cell, if the UE receives SIB change notification, the UE is expected to receive SIB1 from NES cell.

RAN2 to wait for RAN1’s progress whether to support scenario 3.

**RAN2#127**

No consensus for RAN1 case 3 in RAN2.

We can rely on legacy UE behaviour to ensure UE has valid SIB1 for the cell (i.e. UE reacquire SIB1 whenever (re)selecting cell).

Further UE keeps SIB1 updated while on cell via regular SI modification procedure (confirmation of earlier RAN2 agreement).

Once Rel-19 NES UE camps on the NES cell, the UE expects to receive UL WUS configuration updates from the NES Cell, e.g., via legacy SI modification procedures.

Msg 3 based OD-SI procedure is not supported for on-demand SIB1 request in case 2 (for requesting to the NES Cell).

Following example options to handle legacy UEs (i.e. UEs not supporting OD-SIB1) can be considered in normative work. Details and further analysis need to be further discussed in normative work. Other existing options are not excluded.

* Option 1: Legacy UEs bar the OD-SIB1 cell based on cellBarred bit set to barred in MIB.
* Option 2: Legacy UEs bar the OD-SIB1 cell based on no SIB1 indication via ssb-SubcarrierOffset in MIB.
* Option 3: Network includes cells supporting OD-SIB1 to list of excluded cells.

RAN2 understands the NW can avoid impact on legacy RRC connected UE and R19 RRC connected UE due to on-demand SIB1 (e.g. NES cell with OD-SIB1 is measured by legacy RRC\_CONNECTED UE and can be configured as its PSCell/SCells/target cell).

RAN2 conclude that on-demand SIB1 is feasible from RAN2 perspective and recommend normative work of case 2 for on-demand SIB1.

**RAN2#127bis**

We will inherit all agreements made during SI phase to WI phase.

A NES cell can include neighbouring NES cell’s WUS configuration.

NES cell’s WUS configuration, it is included in a new SIB (including its own WUS configuration).

In on-demand SIB1 procedure, the UE considers RACH failure when PREAMBLE\_TRANSMISSION\_COUNTER = preambleTransMax + 1.

The MAC layer will indicate the RACH failure for SI request to upper layers. FFS: after that the UE upper layer will consider the cell as barred.

The legacy UE behaviour can be reused upon on-demand SIB1 acquisition failure, i.e., the NES UE should follow the intraFreqReselection in MIB of NES cell.

A cell for which SIB1 request configuration is available, can periodically broadcast SIB1.

If UE has SIB1 request configuration of a cell, UE needs to check if SIB1 is currently being broadcasted or provided on demand for that cell before requesting SIB1 of that cell.

Legacy UEs bar the OD-SIB1 cell based on no SIB1 indication in MIB e.g. via ssb-SubcarrierOffset. Detailed solution is up to RAN1. If this works, no separate barring bit for R19 NES UEs is introduced.

NES UEs should be allowed to reselect to cells that are prevented from legacy UEs (e.g. by excluded cell list, reselection priorities).

RAN2 will not start the discussion on the issue when the UL WUS configuration update in Cell A is not synchronised with the UL WUS configuration update in the NES cell, unless we’re asked to do that by other WG, e.g. RAN3.

**RAN2#128**

Let’s wait for more RAN1 progress on Kssb discussion.

NES UE with SIB1 request configuration of a NES cell assumes that a NES cell, with SSB containing K\_SSB < 24 for FR1 and K\_SSB < 12 for FR2, will acquire SIB1 as in legacy.

New NES-specific reselection priority parameters for NES UEs are defined for the purpose of prioritizing/deprioritizing a NES frequency.

Introduce new IntraFreqExcludedCellList-NES / InterFreqExcludedCellList-NES IEs enable proper reselection behaviour of legacy and NES UEs.

Reuse legacy cell reselection criterion as trigger condition of OD-SIB1 acquisition. No need to specify other conditions (e.g. a new RSRP threshold).

The existing 1-second rule in the cell reselection criteria is still applied to the triggering condition of UL WUS transmission.

The UE considers the cell as barred after MAC indicates max number of preamble transmission for the OD-SIB1 request.

If MSG2 (ACK) is received, but UE fails to receive SIB1 then the UE may consider this cell as barred, no spec impact.

A UE bars the NES/SIB1 less cell and/or excludes it as a candidate for reselection since the UE had no corresponding UL WUS configuration, the UE would treat this cell as if cell status is “not barred” and consider it as candidate for cell reselection once it has received a UL-WUS configuration to request SIB1 for this cell.

UE considers WUS configuration only valid in directly succeeding cell reselection from cell where UE acquired WUS configuration. FFS on SI validity area rather than cell level.

Wait one cycle of RAN discussion (i.e. to see whether WID is updated or not to handle RRC connected UEs)

Working assumption: UL-WUS configuration in RRC release is not supported.

**RAN2#129**

There is no need for additional barring mechanisms (in addition to the k\_ssb signaling “no SIB1” indication in MIB) to handle legacy to be able to bar cell using OD-SIB1.

Specify the following UE behavior to allow the UEs in RRC\_CONNECTED state to acquire OD-SIB1 when T311 is running:

* When T311 is running, the UE can trigger the OD-SIB1 acquisition procedure with stored UL WUS configuration in SIB-X, if it is still valid.
* The legacy cell selection criteria are reused as the trigger condition of OD-SIB1 acquisition.
* The OD-SIB1 acquisition behavior is same as that of RRC\_IDLE/IANCTIV UEs.

The UE follows the legacy validity principle of stored SIB.

For Rel-19 NES UE in RRC\_CONNECTED, rely on the NW dedicated RRC for SIB1 delivery if searchSpaceSIB1 is not configured. It is legacy UE behavior and no spec change is expected.

SIB-x can be cell specific or area specific, as legacy.

Upon reception of RAR, the UE monitors OD-SIB1 in the window agreed by RAN1.

**RAN2#129bis**

Capture the following understanding in meeting notes: RA on an SpCell can include a cell on which the UE is requesting OD-SIB1. No specification changes needed.

Reuse legacy SSB selection procedure in MAC spec for RA initiated for SIB1 request, i.e. the UE selects any SSB if no SSB is above the configured RSRP threshold. This can be revisited if RAN1 agrees otherwise.

NW ensures that the RRC connected UE has the latest SIB1 (e.g. dedicated RRC message to deliver SIB1 or not configure searchSpaceSIB1), as baseline. UE understands that the stored SIB1 is the latest SIB1.

When the cell supporting on demand SIB1 is broadcasting SIB1 (e.g. upon SIB1 request), legacy UE can camp on the cell if the legacy UE is able to acquire the broadcasted SIB1. No specification impact is foreseen.

Confirm the working assumption that “UL-WUS configuration in RRC release is not supported”.

SIBX that was acquired during RRC connected state can be used for OD-SIB1 request in RLF.

Align with legacy RAR for OSI for OD-SIB1 operation. Legacy RAR MAC PDU subheader with RAPID only to be used as NW acknowledgement for OD-SIB1 request.

The UL WUS configuration includes the IE totalNumberOfRA-Preambles.

Backoff is not applied to OD-SIB1 request when backoff is included in RAR.

Leave this issue (how to handle paging interruption during OD-SIB1 acquisition) to RAN4.

If UE has not received the PDCCH scheduling SIB1 upon the expiry of the SIB1 monitoring window, UE may consider the cell as being barred.

WUS configuration can be associated with a list of cells if the whole WUS configuration is same.

Area id will be used as legacy.

We do not need a separate new triggering condition of OD-SIB1 acquisition.

When timer T311 is running, SIB1 acquisition triggering condition is same as legacy. No additional spec impact is foreseen.

**Adaptation of common channels/signals**

**RAN2#125bis**

From the UE point of view, UE will monitor one PEI/PO every paging DRX cycle, i.e. the UE doesn’t skip PO in paging DRX cycle.

For adaptation of paging occasions in time domain, RAN2 to study a) bundle paging frames and b) extend the values of N to have increased interval between PFs (e.g. T/64, T/128 ...) and compensating decrease in number of PFs by increasing POs per PF.

For Paging adaptation, R2 discusses the following options on compatibility of legacy RRC\_IDLE/RRC\_INACTIVE UE:

* Option 1: Prevent the access of legacy UE via barring;
* Option 2: Separate paging resources for legacy UEs and Rel-19 NES UEs (assuming there are legacy UEs)

**RAN2#127**

Option-a) is about the bundling of PF for R19 NES UEs.

R2 observe that the option-a) and option-b) can be designed to configure the PO:s at same time position.

**RAN2#127bis**

Select option-b as baseline for R19 NES paging enhancement.

R2 should aim at signaling overhead minimization (e.g., Ns=8 and FFS for other larger values)

Allowing legacy and R19 UEs to co-ex in the same PF/PO is possible, based on NW configuration.

Legacy UE is not barred.

Rel-19 UEs only monitor the PO(s) according to Rel-19 paging configuration.

**RAN2#128**

Introduce value for Ns=8. FFS on 16.

Introduce value for N= T/32. FFS on T/64, T/128, T/256.

**RAN2#129**

For N, values smaller than T/32 are not supported.

The maximum possible value for Ns is 8.

Introduce a separate PEI configuration.

Paging adaptations are configured semi-statically and updated via system information update notification.

A new UE capability is added for R19 NES paging enhancement, and the new capability is included in UE-RadioPagingInfo. FFS on whether we have a common capability for all NES features.

RAN2 confirms SSB adaptation in time domain is not supported for RRC idle/inactive UEs and Rel-19 NES-capable UE’s PCell.

RAN2 preference is to keep SMTC based L3 RRM framework and to introduce additional SMTC configuration according to SSB adaptation for L3 RRM measurement on SCell with SSB adaptation.

For L3 measurement, RAN2 assumes the adapted SSB on neighbor cell is measured based on legacy SMTC.

Legacy UEs and UEs non-capable of time domain PRACH adaptation are expected to use legacy PRACH resources per legacy configuration and procedures. No barring is needed.

RAN2 starts CBRA for RACH adaptation.

RAN2 starts 4-step RACH adaptation.

From R2 perspective, not apply time-domain RACH adaptation to RACH resources for MSG1-based SI request.

From R2 perspective, not apply time-domain RACH adaptation to IAB RACH resources.

From R2 perspective, RACH adaptation is not modelled as RA feature(s).

From R2 perspective, RACH partitioning with all the features, i.e. RedCap, SDT, and Slicing, and feature combinations, are supported for PRACH adaption in time domain.

Will follow legacy mechanism regarding how to select RACH resource.

**RAN2#129bis**

For the case when both pei-Config-r17 and pagingAdaptationPEI-Config-r19 are configured, R19 UE supporting paging adaption should monitor PEI according to pagingAdaptationPEI-Config-r19 while other UE should monitor PEI according to pei-Config-r17.

For the case when pei-Config-r17 is configured and pagingAdaptationPEI-Config-r19 is absent, both R19 UE supporting paging adaption and other UE should monitor PEI according to pei-Config-r17.

Paging clustering/bundling/adaptation is not supported/applied in RRC\_CONNECTED.

Not support MAC CE based signalling to indicate SSB adaptation in addition to DCI agreed in RAN1.

For SSB adaptation, multiple additional SMTC configurations are configured to UE via RRC, together with the mapping between SSB burst periodicity and SMTC configuration.

Upon reception of DCI format 2\_9 for SSB burst periodicity switching, UE selects one SMTC configuration accordingly.

**RAN2#130**

Rely on PHY layer specs to capture availability conditions related to usage of additional PRACH resources. It can be revisited if needed after checking PHY running specifications.

A note in TS 38.321 is added to clarify that UE selects only amongst preambles configured for the next valid RO(s) for the selected SSB, when CB-PreamblesPerSSB is configured for additional ROs. Wording of the note can be refined during the running CR review discussion.

Regarding RA type for PRACH adaptation, support only 4-step RA in Rel-19 unless RAN1 decides supporting 2-step RACH this meeting.

RRC connected UE monitors the DCI-based adaptation indication at least once every once every SI modification period.

No need to extend the RA-RNTI space for additional PRACH occasions, i.e. no RAN2 impact for RA-RNTI calculation. RAN2 assumes that f\_id for the additional PRACH resources is reinterpreted as the index of the PRACH occasion in the frequency domain plus the number of FDMed legacy ROs. RAN2 understand there is no MAC impact.

BI is commonly applied to both legacy RO and additional RO.

RACH adaptation is not applied to the following cases (for non-serving cell case): 1) PDCCH order for additional RACH; 2) L3 HO command. 3) LTM CSC MAC-CE; 4) PDCCH order for LTM early UL sync;

RACH adaptation is not applied to BFR.

RAN2 confirms the newly introduced 1-bit indication in DCI 1\_0 for C-RNTI, i.e., PDCCH order, applies to both CBRA and CFRA.