{"text_format":"1","workbook":"xlsx","n_sheets":4,"sheets":["Simulation assumption","KPIs","Results","Figures"],"not_rendered":{"charts":3,"images":0,"macros":1,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Simulation assumption","index":0,"n_rows":28,"n_cols":9,"rows_kept":28,"cut":false,"hidden":false,"merged":[[0,0,0,1],[4,0,6,0]]}
["SLS simulation assumption",null,"NTT DOCOMO","Qualcomm","Mediatek","Mediatek","Mediatek","OPPO","vivo"]
["Parameter","Values"]
["Frequency Range","FR2 @ 30 GHz with SCS 120 kHz"]
["Deployment","\n2-tier model with wrap-around (7 sites, 3 sectors/cells per site)\n",null,"2-tier model without wrap-around"]
["Channel model","UMi With distance-dependent LoS probability function defined in Table 7.4.2-1 in TR 38.901, fast fading and optional LOSsoft;\nwithout UErotation,Oxygen absorption, Time-varying Doppler shift, Explicit ground reflection model and blockage"]
[null,"Whether LOSsoft is modeled or not","NO","Yes","Yes","Yes","Yes","No","No"]
[null,"spatial consistency option (A or B)","A","A","A","A","A","A","A"]
["System BW","80MHz"]
["UE Speed","60km/h (optional), 90km/h (optional), 120km/h (optional)\nOther values are not precluded","60, 90, 120 kmph","60 km/h"," 60, 120 km/hr"," 60, 120 km/hr"," 60, 120 km/hr","90km/h"," 60, 90, 120 km/h"]
["UE distribution","100% outdoor"]
["BS Antenna Configuration"," Antenna setup and port layouts at gNB: (4, 8, 2, 1, 1, 1, 1), (dV, dH) = (0.5, 0.5) λ\nOther assumptions are not precluded."]
["BS Antenna radiation pattern","TR 38.802 Table A.2.1-6, "]
["UE Antenna Configuration","Antenna setup and port layouts at UE: (1, 4, 2, 1, 2, 1, 1), 2 panels (left, right)\nOther assumptions are not precluded"]
["UE Antenna radiation pattern","TR 38.802 Table A.2.1-8, "]
["BS Tx Power","40dBm"]
["Maximum UE Tx Power","23 dBm"]
["BS receiver Noise Figure","7 dB"]
["UE receiver Noise Figure","10 dB"]
["Inter site distance","200m ISD"]
["BS Antenna height","10m"]
["UE Antenna height","1.5 m"]
["UE trajectory model","Option #1, Option #2, or option #3\nReported by companies","Option3","Based on Option 2 in TR 38.343 [2], Section 6.3.1, with modifications based on Option 4 and a minor modification for extended mobility. Refer to section 2.1.1 in R2-2501459 for a detailed discussion of the trajectory model.","Option1","Option1","Option1","Option1","Option1"]
["UE trajectory boundary processing","Option #1, Option #2, or option #3 \nReported by companies","Option3","Option #3 (trajectory termination)","Option2","Option2","Option2","Option3","Option2"]
["L1/L3 filtering","Option #Sliding, Option #Non-sliding\nReported by companies","Sliding","Option #sliding","both","both","both","Option #Sliding","Option1"]
["Measurement period","400ms",null,"400ms"]
["FilterCoefficient",4]
["Number of Tx beams","Reported by companies",32,1,1,1,32,32,"32 Tx beams"]
["Number of Rx beams","Reported by companies",4,1,1,1,4,4,"4 Rx beams per panel"]

{"sheet":"KPIs","index":1,"n_rows":11,"n_cols":8,"rows_kept":11,"cut":false,"hidden":false,"merged":[]}
["Intermediate KPIs","Description/Definition","Mediatek","Mediatek","Mediatek","Mediatek","OPPO","vivo"]
["Average L3 cell RSRP difference (dB)","Average L3 RSRP difference between the predicted and actual L3 cell-level measurement result for each individual point within the PW, and then averaged across all the points in the PW. ","Method: Average cross multiple cells","Method: Average cross multiple cells","Method: Average cross multiple cells","Method: Average cross multiple cells","Method: Average across multiple instances of serving cell of multiple UE trajectories","Method: Average cross multiple cells"]
["Last predicted point L3 cell RSRP difference (dB)","Average L3 RSRP difference between predicted and ideal L3 cell-level measurement result for the last point in PW.",null,null,null,null,"Method: Average cross multiple cells"]
["Multiple predicted point L3 cell RSRP differences (dB)","Average L3 RSRP difference between predicted and ideal L3 cell-level measurement result for each individul point in PW. Multiple values are provided if there are multiple points within the PW."]
["L3 beam RSRP difference(dB)","Average L3 beam-level RSRP difference between predicted and ideal L3 beam-level measurement result for all points in PW."]
["F1 score","2*Precision*Recall/(Precision + Recall)"]
["Precision","n3/(n1+n3)"]
["Recall","n3/(n2+n3)"]
["n1 (false event detection)","it increases by 1 when no real event occurs around a predicted event with ETD, whose range is [0, maximum ETD]"]
["n2 (missed event detection)","it increases by 1 when no event is predicted around a real event with ETD, whose range is [0, maximum ETD]"]
["n3 (true event prediction)","it increases by 1 when a real event occurs around a predicted event with ETD, whose range is [0, maximum ETD] or vice versa"]

{"sheet":"Results","index":2,"n_rows":48,"n_cols":42,"rows_kept":48,"cut":false,"hidden":false,"merged":[[0,36,0,38],[0,39,0,41],[0,0,0,2],[0,3,0,8],[0,9,0,16],[0,17,0,25],[0,26,0,32],[0,33,0,35]]}
["General",null,null,"Variable Settings",null,null,null,null,null,"Configurable/Selectable Simulation Assumption",null,null,null,null,null,null,null,"Model Related Information",null,null,null,null,null,null,null,null,"Intermediate Performance Metrics",null,null,null,null,null,null,"SLS Performance Metrics (Baseline)",null,null,"SLS Performance Metrics (HO Option 1)",null,null,"SLS Performance Metrics(HO Option 2)"]
["Company","Sub-use case","Other factors","Observation window(ms)","Prediction window(ms)","A3 event offset \n(dB)","TTT\n(ms)","max ETD\n(ms)","UE speed\n(km/h)","Spatial consistency","Whether LOSsoft is modeled or not","UE trajectory model","UE trajectory boundary processing","L1/L3 filtering\n(Sliding/Non-sliding)","Use earlier predicted results used as inputs","Number of Tx beams","Number of Rx beams","Model input","Model output/label","Model type","Detail of model","Model complexity\nin a number of model parameters (K)","Model complexity\nin a number of model size (KBytes)","Computational complexity [FLOPs]\n(M)","Training data size in number of samples (K)","Testing data size in number of samples (K)","F1 score","Precision ","Recall"," Average L3 cell RSRP difference (dB)","Last predicted point L3 cell RSRP difference (dB) ","Multiple predicted point L3 cell RSRP differences (dB)","L3 beam RSRP difference(dB)","HO failure rate\n(%)","Total number of HOF per UE per second","Total number of HO attempts per UE per second","HO failure rate\n(%)","Total number of HOF per UE per second","Total number of HO attempts per UE per second","HO failure rate\n(%)","Total number of HOF per UE per second","Total number of HO attempts per UE per second"]
["Name","1/2/3","Additional consideration (e.g. Cell/Cluster-based)","XX","XX","XX","XX","XX","XX","A/B","YES/NO","1/2/3","1/2/3","Sliding/Non-sliding","YES/NO","XX","XX","Number of cell(s),\nMesurement quantity (L1 beam-level, L1-filterd beam-level, L3 cell-level, L3 beam-level measurement results)","Number of cell(s),\nMeasurement quantity (L1 beam-level, L1-filterd beam-level, L3 cell-level, L3 beam-level measurement results)","AI/Non-AI: Method (e.g. RNN,CNN, Sample and hold, Decision tree)","e.g.,model structure and description","XX","XX","XX","XX","XX","XX","XX","XX","XX","XX","[XX, XX, XX..]","XX","XX","XX","XX","XX","XX","XX","XX","XX","XX"]
["NTT DOCOMO",3,"Cluster-based",320,320,2,320,80,60,"A","NO","3",3,"Sliding","NO",32,4,"7 cell, L1-filtered beam-level RSRP","7 cell, L1-filtered beam-level RSRP","AI:Transformer","6 layers Transformer decoder",9590,37589,96.75,361,90,0.92,1,0.85,0.91,null,null,null,24,0.08,0.34,null,null,null,17,0.08,0.44]
["NTT DOCOMO",3,"Cluster-based",320,320,2,320,80,90,"A","NO","3",3,"Sliding","NO",32,4,"7 cell,  L3 cell-level RSRP  ","7 cell,  L3 cell-level RSRP  ","AI:Transformer","6 layers Transformer decoder",9480,37154,95.08,361,90,0.91,1,0.84,1.06,null,null,null,29,0.13,0.45,null,null,null,19,0.11,0.6]
["NTT DOCOMO",3,"Cluster-based",320,320,2,320,80,120,"A","NO","3",3,"Sliding","NO",32,4,"7 cell, L1-filtered beam-level RSRP","7 cell,  L3 cell-level RSRP  ","AI:Transformer","6 layers Transformer decoder",9530,37379,95.64,361,90,0.91,1,0.83,1.1100000000000001,null,null,null,31,0.17,0.54,null,null,null,19,0.15,0.75]
["NTT DOCOMO",3,"Cluster-based",320,320,2,80,80,60,"A","NO","3",3,"Sliding","NO",32,4,"7 cell, L1-filtered beam-level RSRP","7 cell, L1-filtered beam-level RSRP","AI:Transformer","6 layers Transformer decoder",9590,37589,96.75,361,90,0.92,1,0.85,0.91,null,null,null,22,0.09,0.41,null,null,null,16,7.0000000000000007E-2,0.45]
["NTT DOCOMO",3,"Cluster-based",320,320,2,80,80,90,"A","NO","3",3,"Sliding","NO",32,4,"7 cell,  L3 cell-level RSRP  ","7 cell,  L3 cell-level RSRP  ","AI:Transformer","6 layers Transformer decoder",9480,37154,95.08,361,90,0.91,1,0.84,1.06,null,null,null,24,0.13,0.62,null,null,null,18,0.11,0.62]
["NTT DOCOMO",3,"Cluster-based",320,320,2,80,80,120,"A","NO","3",3,"Sliding","NO",32,4,"7 cell, L1-filtered beam-level RSRP","7 cell,  L3 cell-level RSRP  ","AI:Transformer","6 layers Transformer decoder",9530,37379,95.64,361,90,0.91,1,0.83,1.1100000000000001,null,null,null,25,0.17,0.78,null,null,null,19,0.15,0.78]
["Qualcomm",2,"Cell-based","<= 1280",400,2,160,80,60,"A","YES","2",3,"Sliding","NO",8,8,"21 cell, L3 cell-level RSRP","21 cell, L3 cell-level RSRP","AI: Transformer","Encoder-only transformer",1279,9800,null,"3240 trajectories","811 trajectories",0.59,44.22,89.86,null,null,null,null,2.41,null,null,null,null,null,2.82]
["Qualcomm",2,"Cell-based","<= 1280",400,2,160,80,60,"A","YES","2",3,"Sliding","NO",8,8,"21 cell, L3 cell-level RSRP","21 cell, L3 cell-level RSRP","Non-AI:Sample and hold",null,null,null,null,null,null,0.59,41.58,100,null,null,null,null,2.41,null,null,null,null,null,2.98]
["Qualcomm",2,"Cell-based","<= 1280",400,2,320,80,60,"A","YES","2",3,"Sliding","NO",8,8,"21 cell, L3 cell-level RSRP","21 cell, L3 cell-level RSRP","AI: Transformer","Encoder-only transformer",1279,9800,null,"3240 trajectories","811 trajectories",0.47,33.74,76.2,null,null,null,null,1.92,null,null,null,null,null,2.37]
["Qualcomm",2,"Cell-based","<= 1280",400,2,320,80,60,"A","YES","2",3,"Sliding","NO",8,8,"21 cell, L3 cell-level RSRP","21 cell, L3 cell-level RSRP","Non-AI:Sample and hold",null,null,null,null,null,null,0.46,30.08,100,null,null,null,null,1.92,null,null,null,null,null,2.98]
["Ericsson",2,"Cluster-based",400,320,2,320,80,60,"B","YES",3,1,"Sliding","NO",8,1,"21 cells L3 cell level","21 cells L3 cell level","LSTM",null,145,580,0.441,230,1000,0.98299999999999998,"0.971","0.995","0.832",1.19,"-","-",0.11203194346695775,3.2463589618373235E-4,0.28977083333333331,0.75900000000000001,2.0113500000000003E-3,0.26500000000000001,0.1425757709380604,4.0359042292579205E-4,0.28307083333333333]
["Ericsson",2,"Cluster-based",400,320,2,320,80,90,"B","YES",3,1,"Sliding","NO",8,1,"21 cells L3 cell level","21 cells L3 cell level","LSTM",null,64,260,0.155,230,1000,0.98199999999999998,0.96899999999999997,0.995,0.77300000000000002,1.22,"-","-",0.2294386555010374,8.2518568445346025E-4,0.35965416666666666,1.1459420280799535,3.7770487983437785E-3,0.32960208333333335,0.26538904154630216,9.3916758652543898E-4,0.35388333333333333]
["Ericsson",2,"Cluster-based",400,320,2,320,80,120,"B","YES",3,1,"Sliding","NO",8,1,"21 cells L3 cell level","21 cells L3 cell level","LSTM",null,64,260,0.155,230,1000,0.98699999999999999,0.97699999999999998,0.997,0.82199999999999995,1.31,"-","-",0.29352725994012241,1.2484081274328331E-3,0.42531249999999998,1.457442978130528,5.7339450367100298E-3,0.39342500000000002,0.32810087493566648,1.3767181066649508E-3,0.41960208333333332]
["Huawei",2,"Cell-based",320,320,2,320,80,90,"B","NO",1,1,"Non-sliding","NO",64,8,"1 cell, L3 cell-level RSRP  ","1 cell, L3 cell-level RSRP  ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.04,4300,30,0.32,0.38,0.28000000000000003,1.36,null,null,null,70.58,0.41899999999999998,0.59399999999999997,70.58,0.41899999999999998,0.59399999999999997,25,0.105,0.41899999999999998]
["Huawei",2,"Cell-based",320,320,2,240,80,90,"B","NO",1,1,"Non-sliding","NO",64,8,"1 cell, L3 cell-level RSRP  ","1 cell, L3 cell-level RSRP  ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.04,4300,30,0.56000000000000005,0.57999999999999996,0.55000000000000004,1.36,null,null,null,73.680000000000007,0.48899999999999999,0.66300000000000003,73.680000000000007,0.48899999999999999,0.66300000000000003,22.22,0.14000000000000001,0.628]
["Huawei",2,"Cell-based",320,320,2,320,160,90,"B","NO",1,1,"Non-sliding","NO",64,8,"1 cell, L3 cell-level RSRP  ","1 cell, L3 cell-level RSRP  ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.04,4300,30,0.52,0.62,0.44,1.36,null,null,null,70.58,0.41899999999999998,0.59399999999999997,70.58,0.41899999999999998,0.59399999999999997,25,0.105,0.41899999999999998]
["Huawei",2,"Cell-based",320,320,2,240,160,90,"B","NO",1,1,"Non-sliding","NO",64,8,"1 cell, L3 cell-level RSRP  ","1 cell, L3 cell-level RSRP  ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.04,4300,30,0.87,0.89,0.85,1.36,null,null,null,73.680000000000007,0.48899999999999999,0.66300000000000003,73.680000000000007,0.48899999999999999,0.66300000000000003,22.22,0.14000000000000001,0.628]
["Mediatek",2,"Cluster-based",400,320,2,160,80,120,"A","YES",1,2,"Sliding ","NO",32,4,"21 cells, L3 cell-level RSRP","21 cells, L3 cell-level RSRP","AI: CNN","2 layers of convolution layer and 1 FNN layer",52,209.5,10.24,266,133,0.91500000000000004,0.96399999999999997,0.87,0.64,1.22,null,null,18.8,7.1099999999999997E-2,0.378,null,null,null,23.7,5.2400000000000002E-2,0.221]
["Mediatek",2,"Cluster-based",400,320,2,320,80,120,"A","YES",1,2,"Sliding ","NO",32,4,"21 cells, L3 cell-level RSRP","21 cells, L3 cell-level RSRP","AI: CNN","2 layers of convolution layer and 1 FNN layer",52,209.5,10.24,266,133,0.874,0.94099999999999995,0.81599999999999995,0.64,1.22,null,null,23.4,6.2199999999999998E-2,0.26600000000000001,null,null,null,26.6,5.9799999999999999E-2,0.22500000000000001]
["OPPO",2,"cell-based",400,400,2,320,80,90,"A","NO",1,3,"Sliding","NO",32,4,"1 cell, L3 cell-level RSRP","1 cell, L3 cell-level RSRP","AI: LSTM","2LSTM layer+1 dense layer",177,674,0.41,73.400000000000006,37,0.97,0.97,0.97,0.68,1.41,null,null,28.96,9.6000000000000002E-2,0.33,28.42,0.108,0.38,24.2,8.8999999999999996E-2,0.34]
["OPPO",2,"cell-based",400,320,2,320,80,90,"A","NO",1,3,"Sliding","NO",32,4,"1 cell, L3 cell-level RSRP","1 cell, L3 cell-level RSRP","AI: LSTM","2LSTM layer+1 dense layer",177,674,0.41,73.400000000000006,37,0.98,0.96,1,0.69,1.23,null,null,28.96,9.6000000000000002E-2,0.33,28.42,9.6000000000000002E-2,0.34,24.63,8.8999999999999996E-2,0.36]
["vivo",2,"Cell-based",400,320,2,"320","80",60,"A","NO",1,2,"Sliding ","NO",32,"4 per panel","1 cell,L3 cell-level","1 cell,L3 cell-level","AI：LSTM","1 layers of LSTM layer and 1 FNN layer",17,69,0.84499999999999997,400,100,0.96799999999999997,0.93899999999999995,1,0.87,1.6160000000000001,"[0.230, 0.578, 1.057, 1.616]"]
["vivo",2,"Cell-based",400,320,2,"320","80",60,"A","NO",1,2,"Sliding ","NO",32,"4 per panel","1 cell,L3 cell-level","1 cell,L3 cell-level","Non-AI: Sample and hold","Replace the\npredicted measurement with the last observation measurement",null,null,null,400,100,0.94699999999999995,0.9,1,1.7729999999999999,2.78,"[0.732, 1.446, 2.133, 2.780]"]
["vivo",2,"Cell-based",400,320,2,"320","80",90,"A","NO",1,2,"Sliding ","NO",32,"4 per panel","1 cell,L3 cell-level","1 cell,L3 cell-level","AI：LSTM","1 layers of LSTM layer and 1 FNN layer",17,69,0.84499999999999997,400,100,0.96599999999999997,0.93500000000000005,1,1.1719999999999999,2.1480000000000001,"[0.316, 0.800, 1.425, 2.148]",null,5.98,2.1000000000000001E-2,0.35049999999999998,5.1100000000000003,1.8599999999999998E-2,0.3649,3.77,1.4E-2,0.3705]
["vivo",2,"Cell-based",400,320,2,"320","80",90,"A","NO",1,2,"Sliding ","NO",32,"4 per panel","1 cell,L3 cell-level","1 cell,L3 cell-level","Non-AI: Sample and hold","Replace the\npredicted measurement with the last observation measurement",null,null,null,400,100,0.93,0.86899999999999999,1,2.1869999999999998,3.3959999999999999,"[0.918, 1.804, 2.628, 3.396]"]
["vivo",2,"Cell-based",400,320,2,"320","80",120,"A","NO",1,2,"Sliding ","NO",32,"4 per panel","1 cell,L3 cell-level","1 cell,L3 cell-level","AI：LSTM","1 layers of LSTM layer and 1 FNN layer",17,69,0.84499999999999997,400,100,0.96699999999999997,0.93600000000000005,1,1.36,2.468,"[0.382, 0.936, 1.655, 2.468]"]
["vivo",2,"Cell-based",400,320,2,"320","80",120,"A","NO",1,2,"Sliding ","NO",32,"4 per panel","1 cell, L3 cell-level","1 cell, L3 cell-level","Non-AI: Sample and hold","Replace the\npredicted measurement with the last observation measurement",null,null,null,400,100,0.94,0.88600000000000001,1,2.3820000000000001,3.6850000000000001,"[1.013, 1.969, 2.862, 3.685]"]
["Xiaomi",2,"Cell-based",800,400,2,320,80,90,"A","No","1",2,"Sliding ","NO",8,4,"1 cell, L3 cell-level RSRP  ","1 cell, L3 cell-level RSRP  ","AI-GRU","1 layer of GRU  based on encoder-decoder with 1 layer of FNN",696.35900000000004,8210,44.280239999999999,1673.614,211.82300000000001,0.83079999999999998,0.71179999999999999,0.99739999999999995,2.4569999999999999,4.234,"[0.721,1.540,2.453,3.337,4.234]"]
["Xiaomi",2,"Cell-based",800,320,2,320,80,90,"A","No","1",2,"Sliding ","NO",8,4,"1 cell, L3 cell-level RSRP  ","1 cell, L3 cell-level RSRP  ","AI-GRU","1 layer of GRU  based on encoder-decoder with 1 layer of FNN",696.35900000000004,8210,39.98968,1674.4359999999999,211.90199999999999,0.83850000000000002,0.72360000000000002,0.99660000000000004,2.0750000000000002,3.5139999999999998,"[0.695,1.553,2.537,3.514]"]
["Xiaomi",2,"Cell-based",720,240,2,320,80,90,"A","No","1",2,"Sliding ","NO",8,4,"1 cell, L3 cell-level RSRP  ","1 cell, L3 cell-level RSRP  ","AI-GRU","1 layer of GRU  based on encoder-decoder with 1 layer of FNN",696.35900000000004,8210,37.277880000000003,1676.076,212.06200000000001,0.90900000000000003,0.83620000000000005,0.99570000000000003,1.591,2.5409999999999999,"[0.6912,1.5468,2.541]"]
["Xiaomi",2,"Cell-based",480,160,2,320,80,90,"A","No","1",2,"Sliding ","NO",8,4,"1 cell, L3 cell-level RSRP  ","1 cell, L3 cell-level RSRP  ","AI-GRU","1 layer of GRU  based on encoder-decoder with 1 layer of FNN",696.35900000000004,8210,24.85192,1679.471,212.358,0.94779999999999998,0.90859999999999996,0.99050000000000005,1.1839999999999999,1.6379999999999999,"[0.728,1.638]"]
["CMCC",2,"Cluster-based","800",400,2,320,80,"90","A","YES","1",2,"Sliding ","NO",32,4,"21 cells, L3 cell-level RSRP","21 cells, L3 cell-level RSRP","AI: LSTM",null,5600,64140,55.09,194,48,0.95350000000000001,0.95030000000000003,0.94720000000000004]
["CATT",2,"Cluster-based","400",400,2,320,80,"90","A","YES",1,2,"Sliding ","NO",32,4,"21 cells, L3 cell-level RSRP","21 cells, L3 cell-level RSRP","LSTM autoencoder","2 layers of LSTM layer and 1 DNN layer","5601K","64138KBytee","23.44M","194K","48K",0.89249999999999996,0.89459999999999995,0.89049999999999996,1.4590000000000001]
["CATT",2,"Cluster-based","400",400,2,320,80,"90","A","YES",1,2,"Sliding ","NO",32,4,"21 cells, L3 cell-level RSRP","21 cells, L3 cell-level RSRP","LSTM autoencoder","2 layers of LSTM layer and 1 DNN layer","5601K","64138KBytee","23.44M","194K","48K",0.89249999999999996,0.89459999999999995,0.89049999999999996,1.4590000000000001]
["ZTE",2,"Cell-based","800",400,2,320,80,"120","A","NO","3",2,"Non-sliding","NO",32,4,"1 cell, L3 cell-level RSRP ","1 cell, L3 cell-level RSRP ","AI: LSTM","2 LSTM layer + 1 Full connection output layer",792.83900000000006,3097.03,7.9580000000000002,90,7.5,"0.6136 (using all predicted L3 RSRP in TTT )\n0.7347 (using 1 real L3 RSRP + predicted L3 RSRP)\n0.8665 (using 2 real L3 L3 RSRP + predicted L3 RSRP)","0.6051 (using all predicted L3 RSRP in TTT )\n0.7223 (using 1 real L3 RSRP + predicted L3 RSRP)\n0.8570 (using 2 real L3 L3 RSRP + predicted L3 RSRP)","0.6226 (using all predicted L3 RSRP in TTT )\n0.7477 (using 1 real L3 RSRP + predicted L3 RSRP)\n0.8764 (using 2 real L3 L3 RSRP + predicted L3 RSRP)",null,0.94]
["Interdigital",2,null,400,400,2,320,80,90,"A","Yes",1,3,"Sliding","No",16,4,"21 cells, L3 cell-level RSRPs","21 cells, L3 cell-level RSRPs","AI:CNN",null,70,null,1.4570000000000001,16.399999999999999,4.0999999999999996,0.94710000000000005,0.95550000000000002,0.93879999999999997,0.1414,0.29199999999999998,"[0.022, 0.065, 0.126, 0.202, 0.292] "]
["Samsung",2,"Cell-based","800",400,2,320,80,"30","B","YES","3","3","Sliding ","NO",32,4,"1 cell, L3 cell-level RSRP  ","1 cell, L3 cell-level RSRP  ","LSTM autoencoder","2 LSTM layers for encoder \n2 LSTEM layers + 3 dense layers for decoder",4.5,200,0.02,31,0.9,0.79790000000000005,0.93020000000000003,0.69950000000000001]
["Samsung",2,"Cell-based","800",400,2,320,80,"60","B","YES","3","3","Sliding ","NO",32,4,"1 cell, L3 cell-level RSRP  ","1 cell, L3 cell-level RSRP  ","LSTM autoencoder","2 LSTM layers for encoder \n2 LSTEM layers + 3 dense layers for decoder",4.5,200,0.02,31,0.9,0.80259999999999998,0.91879999999999995,0.71340000000000003]
["Samsung",2,"Cell-based","800",400,2,320,80,"90","B","YES","3","3","Sliding ","NO",32,4,"1 cell, L3 cell-level RSRP  ","1 cell, L3 cell-level RSRP  ","LSTM autoencoder","2 LSTM layers for encoder \n2 LSTEM layers + 3 dense layers for decoder",4.5,200,0.02,31,0.9,0.81699999999999995,0.90820000000000001,0.74339999999999995]
["Samsung",2,"Cell-based","800",400,2,320,80,"30","B","YES","3","3","Sliding ","NO",32,4,"1 cell, L3 cell-level RSRP  ","1 cell, L3 cell-level RSRP  ","LSTM autoencoder","2 LSTM layers for encoder \n2 LSTEM layers + 3 dense layers for decoder",4.5,200,0.02,31,0.9,0.79790000000000005,0.93020000000000003,0.69950000000000001]
["Samsung",2,"Cell-based","800",400,2,320,80,"60","B","YES","3","3","Sliding ","NO",32,4,"1 cell, L3 cell-level RSRP  ","1 cell, L3 cell-level RSRP  ","LSTM autoencoder","2 LSTM layers for encoder \n2 LSTEM layers + 3 dense layers for decoder",4.5,200,0.02,31,0.9,0.80259999999999998,0.91879999999999995,0.71340000000000003]
["Samsung",2,"Cell-based","800",400,2,320,80,"90","B","YES","3","3","Sliding ","NO",32,4,"1 cell, L3 cell-level RSRP  ","1 cell, L3 cell-level RSRP  ","LSTM autoencoder","2 LSTM layers for encoder \n2 LSTEM layers + 3 dense layers for decoder",4.5,200,0.02,31,0.9,0.81699999999999995,0.90820000000000001,0.74339999999999995]
["Samsung",2,"Legacy (No prediction)",null,0,2,320,null,"30","B","YES","3","3","Sliding ","NO",32,4]
["Samsung",2,"Legacy (No prediction)",null,0,2,320,null,"60","B","YES","3","3","Sliding ","NO",32,4]
["Samsung",2,"Legacy (No prediction)",null,0,2,320,null,"90","B","YES","3","3","Sliding ","NO",32,4]

{"sheet":"Figures","index":3,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}