**3GPP TSG-RAN WG2 Meeting #131 *R2-250xxxx***

**Bengaluru, Indian, August 25 – 29, 2025**

|  |
| --- |
| *CR-Form-v12.3* |
| **CHANGE REQUEST** |
|  |
|  | **38.304** | **CR** | **0442** | **rev** | **1** | **Current version:** | **18.4.0** |  |
|   |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  |  |
|  |  |
| ***Source to WG:*** | Apple (Rapporteur) |
| ***Source to TSG:*** |  R2 |
|  |  |
| ***Work item code:*** | Netw\_Energy\_NR\_enh-Core  |  | ***Date:*** | 2025-09-01 |
|  |  |  |  |  |
| ***Category:*** | B |  | ***Release:*** | Rel-19 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19) Rel-20 (Release 20)* |
|  |  |
| ***Reason for change:*** | Introduction of Rel-19 network energy saving to TS 38.304. |
|  |  |
| ***Summary of change:*** | This CR introduces Release-19 Network Energy Savings Enhancements for NR in TS 38.304.  |
|  |  |
| ***Consequences if not approved:*** | Release-19 network energy saving is not supported |
|  |  |
| ***Clauses affected:*** | 3.1, 3.2, 5.2.4.1, 5.3.1, 7.1, 7.2.1 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** | **X** |  |  Other core specifications  | TS 38.300 CR1013TS 38.331 CR5428TS 38.321 CR2110 |
| ***affected:*** |  | **X** |  Test specifications |  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications |  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

First change

## 3.1 Definitions

For the purposes of the present document, the following terms and definitions apply:

**2Rx XR UE**:two antenna port XR UE as specified in TS 38.101-1 [15].

**Acceptable Cell**: A cell that satisfies certain conditions as specified in 4.5.

**Allowed CAG list**: A per-PLMN list of CAG Identifiers the UE is allowed to access (see TS 23.501 [10])**.**

**Available PLMN(s)**: One or more PLMN(s) for which the UE has found at least one cell and read its PLMN identity(ies).

**Available SNPN(s)**: One or more SNPN(s) for which the UE has found at least one cell and read its SNPN identity(ies).

**Barred Cell**: A cell a UE is not allowed to camp on.

**CAG cell**: A cell broadcasting at least one Closed Access Group Identifier.

**Camped on a cell**: UE has completed the cell selection/reselection process and has chosen a cell. The UE monitors system information and (in most cases) paging information.

**Camped on any cell**: UE is in idle mode and has completed the cell selection/reselection process and has chosen a cell irrespective of PLMN identity.

**Closed Access Group Identifier**: Identifier of a CAG within a PLMN.

**Commercial Mobile Alert System**: Public Warning System that delivers *Warning Notifications* provided by *Warning Notification Providers* to CMAS capable UEs.

**Earth-fixed cell:** An NTN cell fixed with respect to a certain geographic area on the earth all the time. It can be provisioned by beam(s) continuously covering the same geographical areas all the time (e.g., the case of GSO satellites).

**Earth-moving cell**: An NTN cell moving on the ground. It can be provisioned by beam(s) whose coverage area slides over the Earth surface (e.g., the case of NGSO satellites generating fixed or non-steerable beams).

**eCall Only Mode**: A UE configuration option that allows the UE to register at 5GC and register in IMS to perform only eCall Over IMS, and a non-emergencyIMS call for test and/or terminal reconfiguration services.

**EHPLMN**:Any of the PLMN entries contained in the Equivalent HPLMN list TS 23.122 [9].

**Equivalent PLMN list**:List of PLMNs considered as equivalent by the UE for cell selection, cell reselection, and handover according to the information provided by the NAS.

**Equivalent SNPN list**:List of SNPNs considered as equivalent by the UE for cell selection, cell reselection, and handover according to the information provided by the NAS.

**eRedCap UE**:A UE with enhanced reduced capabilities as specified in clause 4.2.22 in TS 38.306 [24].

**Home PLMN**: A PLMN where the Mobile Country Code (MCC) and Mobile Network Code (MNC) of the PLMN identity are the same as the MCC and MNC of the IMSI.

**HSDN cell**: A cell that has higher priority than other cells for cell reselection for HSDN capable UE in a High-mobility state.

**Mobile-IAB cell**: As defined in TS 38.300 [2].

**Network Identifier**: Identifier of an SNPN in combination with a PLMN ID (TS 23.501 [10]).

**Non-Public Network**: A network deployed for non-public use, as defined in TS 22.261 [12].

**Non-terrestrial network**: An NG-RAN consisting of gNBs, which provides non-terrestrial NR access to UEs by means of an NTN payload embarked on an airborne or space-borne NTN vehicle and an NTN Gateway.

**NR sidelink communication**: AS functionality enabling at least V2X Communication as defined in TS 23.287 [16] and/or A2X Communication as defined in TS 23.256 [26], and ProSe communication (including ProSe non-Relay, UE-to-Network Relay communication and, UE-to-UE Relay communication including UE-to-UE Relay communication with integrated discovery) as defined in TS 23.304 [22], between two or more nearby UEs, using NR technology but not traversing any network node.

**NR sidelink discovery**: AS functionality enabling ProSe non-Relay Discovery, ProSe UE-to-Network Relay discovery and ProSe UE-to-UE Relay discovery for Proximity based Services as defined in TS 23.304 [22] between two or more nearby UEs, using NR technology but not traversing any network node.

**Paging adaptation**: As defined in TS 38.300 [2].

**Process**: A local action in the UE invoked by an RRC procedure or an RRC\_IDLE or RRC\_INACTIVE state procedure.

**Quasi-Earth fixed cell**: An NTN cell fixed with respect to a certain geographic area on the earth during a certain time duration. It can be provisioned by beam(s) covering one geographic area for a limited period and a different geographic area during another period (e.g., the case of NGSO satellites generating steerable beams).

**Radio Access Technology**: Type of technology used for radio access, for instance NR or E-UTRA.

**Ranging/Sidelink Positioning**: AS functionality enabling ranging-based services and sidelink positioning as defined in TS 23.586 [25].

**RedCap UE:** A UE with reduced capabilities as specified in clause 4.2.21 in TS 38.306 [24].

**Registration Area**: (NAS) registration area is an area in which the UE may roam without a need to perform location registration, which is a NAS procedure.

**Registered PLMN**: This is the PLMN on which certain Location Registration outcomes have occurred, as specified in TS 23.122 [9].

**Registered SNPN**: This is the SNPN on which certain Location Registration outcomes have occurred, as specified in TS 23.122 [9].

**Reserved Cell**: A cell on which camping is not allowed, except for particular UEs, if so indicated in the system information.

**Selected PLMN**: This is the PLMN that has been selected by the NAS, either manually or automatically.

**Selected SNPN**: This is the SNPN that has been selected by the NAS, either manually or automatically.

**Serving cell**: The cell on which the UE is camped.

**Sidelink**: UE to UE interface for V2X sidelink communication defined in TS 23.287[16].

**SNPN Access Mode**: Mode of operation wherein UE only selects SNPNs (as defined in TS 23.501 [10]).

**SNPN identity**: An identifier of an SNPN comprising of a PLMN ID and an NID combination.

**Strongest cell**: The cell on a particular frequency that is considered strongest according to the layer 1 cell search procedure (TS 38.213 [4], TS 38.215 [11]).

**Suitable Cell**: This is a cell on which a UE may camp. For NR cell, the criteria are defined in clause 4.5, for E-UTRA cell in TS 36.304 [7].

**U2N Relay UE**: a UE that provides functionality to support connectivity to the network for U2N Remote UE(s).

**U2N Remote UE**: a UE that communicates with the network via a U2N Relay UE.

**U2U Relay UE**: a UE that provides functionality to support connectivity for U2U Remote UE(s).

**U2U Remote UE**: a UE that communicates with other UE(s) via a U2U Relay UE.

**V2X sidelink communication**: AS functionality enabling V2X Communication as defined in TS 23.285 [17], between nearby UEs, using E-UTRA technology but not traversing any network node.

Next change

## 3.2 Abbreviations

For the purposes of the present document, the abbreviations given in TR 21.905 [1] and the following apply. An abbreviation defined in the present document takes precedence over the definition of the same abbreviation, if any, in TR 21.905 [1].

AS Access Stratum

ATG Air To Ground

CAG Closed Access Group

CAG-ID Closed Access Group Identifier

CMAS Commercial Mobile Alert System

CN Core Network

DCI Downlink Control Information

DRX Discontinuous Reception

DTX Discontinuous Transmission

eDRX Extended DRX

ETWS Earthquake and Tsunami Warning System

E-UTRA Evolved UMTS Terrestrial Radio Access

E-UTRAN Evolved UMTS Terrestrial Radio Access Network

GIN Group ID for Network selection

H-SFN Hyper System Frame Number

HRNN Human-Readable Network Name

HSDN High Speed Dedicated Network

IAB Integrated Access and Backhaul

IMSI International Mobile Subscriber Identity

L2 Layer-2

MBS Multicast/Broadcast Services

MBS FSAI MBS Frequency Selection Area Identity

MCC Mobile Country Code

MCCH MBS Control Channel

MICO Mobile Initiated Connection Only

MRB MBS Radio Bearer

MTCH MBS Traffic Channel

NAS Non-Access Stratum

NCR Network-Controlled Repeater

NCR-Fwd NCR Forwarding

NCR-MT NCR Mobile Termination

NES Network Energy Savings

NID Network Identifier

NPN Non-Public Network

NR NR Radio Access

NSAG Network Slice AS Group

NTN Non-Terrestrial Network

OD-SIB1 On-demand SIB1

PEI Paging Early Indication

PEI-O Paging Early Indication-Occasion

PH Paging Hyperframe

PLMN Public Land Mobile Network

PTW Paging Time Window

RAT Radio Access Technology

RNA RAN-based Notification Area

RNAU RAN-based Notification Area Update

RRC Radio Resource Control

SDT Small Data Transmission

SL Sidelink

SNPN Stand-alone Non-Public Network

TN Terrestrial Network

TRS Tracking Reference Signal

U2N UE-to-Network

U2U UE-to-UE

UAC Unified Access Control

UE User Equipment

UMTS Universal Mobile Telecommunications System

VSAT Very Small Aperture Terminal

V2X Vehicle to Everything

Next change

#### 5.2.4.1 Reselection priorities handling

Absolute priorities of different NR frequencies or inter-RAT frequencies may be provided to the UE in the system information, in the *RRCRelease* message, or by inheriting from another RAT at inter-RAT cell (re)selection. In the case of system information, an NR frequency or inter-RAT frequency may be listed without providing a priority (i.e. the field *cellReselectionPriority* is absent for that frequency). If any fields with *cellReselectionPriority* or *nsag-CellReselectionPriority* are provided in dedicated signalling, the UE shall ignore any fields with *cellReselectionPriority* and *nsag-CellReselectionPriority* provided in system information.

When UE is in camped normally state, if it supports slice-based cell reselection and has received the network slice(s) and NSAG information from NAS to be used for cell reselection, UE shall derive reselection priorities according to clause 5.2.4.11.

NOTE 00: UE derives reselection priorities according to clause 5.2.4.11 also in case *SIB16* (see TS 38.331 [3]) is not broadcast in the camped cell.

If dedicated frequency priority parameters (*odsib1-CellReselectionPriority*, *odsib1-CellReselectionSubPriority*) are provided in system information, the UE supporting OD-SIB1 ignores the *cellReselectionPriority* and *cellReselectionSubPriority* in the system information and applies the dedicated ones to determine frequency prioritization. If *intraFreqODSIB1-ExcludedCellList* is provided in system information, the UE supporting OD-SIB1 ignores *intraFreqExcludedCellList* and does not consider the cell(s) (if any) in *intraFreqODSIB1-ExcludedCellList* as candidates for cell reselection. If *interFreqODSIB1-ExcludedCellList* is provided in system information, the UE supporting OD-SIB1 ignores *interFreqExcludedCellList* and does not consider the cell(s) (if any) in *interFreqODSIB1-ExcludedCellList* as candidates for cell reselection.

If UE is in *camped on any cell* state, UE shall only apply the priorities provided by system information from current cell, and the UE preserves priorities provided by dedicated signalling and *deprioritisationReq* received in *RRCRelease* unless specified otherwise. When the UE in camped normally state, has only dedicated priorities other than for the current frequency, the UE shall consider the current frequency to be the lowest priority frequency (i.e. lower than any of the network configured values). When the HSDN capable UE is in High-mobility state, the UE shall always consider the HSDN cells to be the highest priority (i.e., higher than any other network configured priorities). When the HSDN capable UE is not in High-mobility state, the UE shall always consider HSDN cells to be the lowest priority (i.e., lower than any other network configured priorities). If the UE is configured to perform both NR sidelink communication and V2X sidelink communication, the UE may consider the frequency providing both NR sidelink communication configuration and V2X sidelink communication configuration to be the highest priority. If the UE is configured to perform NR sidelink communication and not perform V2X communication, the UE may consider the frequency providing NR sidelink communication configuration to be the highest priority. If the UE is configured to perform V2X sidelink communication and not perform NR sidelink communication, the UE may consider the frequency providing V2X sidelink communication configuration to be the highest priority. If the UE is configured to perform ranging/sidelink positioning, the UE may consider the frequency providing ranging/sidelink positioning configuration to be the highest priority.

A UE on a vehicle with a mobile-IAB cell may consider the frequency for which a mobile-IAB cell is the best cell to be the highest priority. The UE identifies a mobile-IAB cell by *mobileIAB-Cell* in SIB1 (see TS 38.331 [3]). The UE may narrow its search scope for mobile-IAB cell(s) by *mobileIAB-CellList* if broadcasted in SIB4 (see TS 38.331 [3]). A non-mobile-IAB cell may be excluded from this mobile IAB frequency prioritization for up to 300 seconds.

NOTE 0a: The frequency only providing the anchor frequency configuration should not be prioritized for V2X service during cell reselection, as specified in TS 38.331[3].

NOTE 0b: When UE is configured to perform NR sidelink communication or V2X sidelink communication performs cell reselection, it may consider the frequencies providing the intra-carrier and inter-carrier configuration have equal priority in cell reselection.

NOTE 0c: The prioritization among the frequencies which UE considers to be the highest priority frequency is left to UE implementation unless otherwise stated.

NOTE 0d: The UE is configured to perform V2X sidelink communication or NR sidelink communication, if it has the capability and is authorized for the corresponding sidelink operation.

NOTE 0e: When UE is configured to perform both NR sidelink communication and V2X sidelink communication, but cannot find a frequency which can provide both NR sidelink communication configuration and V2X sidelink communication configuration, UE may consider the frequency providing either NR sidelink communication configuration or V2X sidelink communication configuration to be the highest priority.

NOTE 0f: Void.

NOTE 0g: How the UE determines itself to be on a vehicle with a mobile-IAB cell is left to the UE's implementation.

The UE shall only perform cell reselection evaluation for NR frequencies and inter-RAT frequencies that are given in system information and for which the UE has a priority provided.

If the MBS broadcast capable UE is receiving or interested to receive an MBS broadcast service(s) and can only receive this MBS broadcast service(s) by camping on a frequency on which it is provided, the UE may consider that frequency to be the highest priority during the MBS broadcast session as specified in TS 38.300 [2] as long as the two following conditions are fulfilled:

1) SIB1 scheduling information of the cell reselected by the UE due to frequency prioritization for MBS contains SIB20;

2) Either:

- One or more MBS FSAI(s) of that frequency is indicated in SIB21 of the serving cell and the same MBS FSAI(s) is also indicated for this MBS broadcast service in MBS User Service Description (USD) as specified in TS 26.517 [20], or

- SIB21 is not provided in the serving cell and that frequency is included in the USD of this service, or

- SIB21 is provided in the serving cell but does not provide the frequency mapping for the concerned service, and that frequency is included in the USD of this service.

NOTE 0g: It is up to UE implementation which frequency to select, when the USD provides multiple frequencies for the service the UE is interested in.

If the MBS broadcast capable UE is receiving or interested to receive an MBS broadcast service, the UE may consider cell reselection candidate frequencies at which it cannot receive the MBS broadcast service to be of the lowest priority during the MBS broadcast session as specified in TS 38.300 [2], as long as SIB1 scheduling information of the cell contains SIB20 on the MBS frequency which the UE monitors and as long as the condition 2) above is fulfilled for the serving cell.

NOTE 0h: Example scenarios in which such down-prioritisation may be needed include the cases where camping is not possible for the UE on the MBS broadcast frequency (e.g. the MBS broadcast frequency belongs to a PLMN different from UE's registered PLMN) while the UE can receive the MBS broadcast service when camped on another frequency than the MBS broadcast frequency or current frequency.

NOTE 0i: The frequency prioritization for MBS broadcast, NR sidelink communication, or V2X sidelink communication may override the re-selection priorities for slice-based cell reselection.

In case UE receives *RRCRelease* with *deprioritisationReq*, UE shall consider current frequency and stored frequencies due to the previously received *RRCRelease* with *deprioritisationReq* or all the frequencies of NR to be the lowest priority frequency (i.e. lower than any of the network configured values) while T325 is running irrespective of camped RAT. The UE shall delete the stored deprioritisation request(s) when a PLMN selection or SNPN selection is performed on request by NAS (TS 23.122 [9]).

NOTE 1: UE should search for a higher priority layer for cell reselection as soon as possible after the change of priority. The minimum related performance requirements specified in TS 38.133 [8] are still applicable.

NOTE 1a: The UE does not consider MBS broadcast, NR sidelink communication or V2X sidelink communication functionality to replace cell reselection priorities caused by HSDN or *deprioritisationReq* functionality.

The UE shall delete priorities provided by dedicated signalling when:

- the UE enters a different RRC state; or

- the optional validity time of dedicated priorities (T320) expires; or

- the UE receives an *RRCRelease* message with the field *cellReselectionPriorities* absent; or

- a PLMN selection or SNPN selection is performed on request by NAS (TS 23.122 [9]).

NOTE 2: Equal priorities between RATs are not supported.

The UE shall not consider any exclude-listed cells as candidate for cell reselection.

The UE shall consider only the allow-listed cells, if configured, as candidates for cell reselection.

NCR-MT may be configured with additional allowed cell list and/or forbidden cell list, see TS 38.300 [2]. The NCR-MT shall consider only the allowed cell list, if configured by OAM as candidates for cell reselection (ignore above exclude-listed cells and/or allow-listed cells). The NCR-MT shall not consider the cells for cell reselection in the forbidden cell list, if configured by OAM.

The UE in RRC\_IDLE state shall inherit the priorities provided by dedicated signalling and the remaining validity time (i.e. T320 in NR and E-UTRA), if configured, at inter-RAT cell (re)selection.

NOTE 3: The network may assign dedicated cell reselection priorities for frequencies not configured by system information.

Next change

### 5.3.1 Cell status and cell reservations

Cell status and cell reservations are indicated in the *MIB* or *SIB1* message as specified in TS 38.331 [3] by means of the following fields:

- *cellBarred* (IE type: "barred" or "not barred")
Indicated in *MIB* message. In case of multiple PLMNs or NPNs indicated in *SIB1*, this field is common for all PLMNs and NPNs. This field is ignored by UEs supporting NTN for NTN access, or by UEs supporting ATG for ATG access.

*- cellBarredATG* (IE type: "barred" or "not barred")
Indicated in *SIB1* message. In case of multiple PLMNs or NPNs indicated in *SIB1*, this field is common for all PLMNs and NPNs. This field is only applicable to ATG UEs.

*-* *cellBarred2RxXR* (IE type: "barred")
Indicated in *SIB1* message. In case of multiple PLMNs or NPNs indicated in *SIB1*, this field is common for all PLMNs and NPNs. This field is only applicable to 2Rx XR UEs.

- *cellBarred-eRedCap1Rx* (IE type: "barred" or "not barred")
Indicated in *SIB1* message. In case of multiple PLMNs or NPNs indicated in *SIB1*, this field is common for all PLMNs and NPNs. This field is only applicable to eRedCap UEs.

- *cellBarred-eRedCap2Rx* (IE type: "barred" or "not barred")
Indicated in *SIB1* message. In case of multiple PLMNs or NPNs indicated in *SIB1*, this field is common for all PLMNs and NPNs. This field is only applicable to eRedCap UEs.

- *cellBarredFixedVSAT* (IE type: "barred" or "not barred")
Indicated in *SIB1* message. In case of multiple PLMNs indicated in *SIB1*, this field is common for all PLMNs. This field is only applicable to VSAT UEs using NTN access.

- *cellBarredMobileVSAT* (IE type: "barred" or "not barred")
Indicated in *SIB1* message. In case of multiple PLMNs indicated in *SIB1*, this field is common for all PLMNs. This field is only applicable to VSAT UEs using NTN access.

- *cellBarredNES* (IE type: "not barred")
Indicated in *SIB1* message. In case of multiple PLMNs or NPNs indicated in *SIB1*, this field is common for all PLMNs and NPNs. This field is only applicable to UEs indicating any of the values in *nes-CellDTX-DRX* as specified in TS 38.306 [24].

- *cellBarredNTN* (IE type: "barred" or "not barred")
Indicated in *SIB1* message. In case of multiple PLMNs indicated in *SIB1*, this field is common for all PLMNs. This field is ignored if the UE does not support NTN access.

- *cellBarredRedCap1Rx* (IE type: "barred" or "not barred")
Indicated in *SIB1* message. In case of multiple PLMNs or NPNs indicated in *SIB1*, this field is common for all PLMNs and NPNs. This field is only applicable to RedCap UEs.

- *cellBarredRedCap2Rx* (IE type: "barred" or "not barred")
Indicated in *SIB1* message. In case of multiple PLMNs or NPNs indicated in *SIB1*, this field is common for all PLMNs and NPNs. This field is only applicable to RedCap UEs.

- *cellReservedForOperatorUse* (IE type: "reserved" or "not reserved")
Indicated in *SIB1* message*.* In case of multiple PLMNs or NPNs indicated in *SIB1*, this field is specified per PLMN or per SNPN.

- *cellReservedForOtherUse* (IE type: "true")
Indicated in *SIB1* message. In case of multiple PLMNs indicated in *SIB1*, this field is common for all PLMNs.

*- cellReservedForFutureUse* (IE type: "true")
Indicated in *SIB1* message. In case of multiple PLMNs or NPNs indicated in *SIB1*, this field is common for all PLMNs and NPNs.

NOTE 0: IAB-MT ignores the *cellBarred*, *cellReservedForOperatorUse, cellReservedForFutureUse,* and *intraFreqReselection* (i.e. treats *intraFreqReselection* as if it was set to *allowed*) as defined in TS 38.331 [3]. IAB-MT also ignores *cellReservedForOtherUse* for cell barring determination (i.e. NPN capable IAB-MT considers *cellReservedForOtherUse* for determination of an NPN-only cell) as defined in TS 38.331 [3].

NOTE 0a: NCR-MT ignores the *cellBarred*, *cellReservedForOperatorUse, cellReservedForFutureUse,* and *intraFreqReselection* (i.e. treats *intraFreqReselection* as if it was set to *allowed*) as defined in TS 38.331 [3]. NCR-MT also ignores *cellReservedForOtherUse* for cell barring determination (i.e. NPN capable NCR-MT considers *cellReservedForOtherUse* for determination of an NPN-only cell) as defined in TS 38.331 [3].

- *halfDuplexRedCapAllowed* (IE type: "true")
Indicated in *SIB1* message. In case of multiple PLMNs or NPNs indicated in *SIB1*, this field is common for all PLMNs and NPNs. This field is only applicable to (e)RedCap UEs.

- *iab-Support* (IE type: "true")
Indicated in *SIB1* message. In case of multiple PLMNs or NPNs indicated in *SIB1*, this field is specified per PLMN or per SNPN. This field is only applicable to IAB-MT.

- *ncr-Support* (IE type: "true")
Indicated in *SIB1* message. In case of multiple PLMNs or NPNs indicated in *SIB1*, this field is common for all PLMNs and NPNs. This field is only applicable to NCR-MT.

- *mobileIAB-Support* (IE type: "true")
Indicated in *SIB1* message. In case of multiple PLMNs or NPNs indicated in *SIB1*, this field is specified per PLMN or per SNPN. This field is only applicable to mobile IAB-MT.

When cell status is indicated as "not barred" and "not reserved" for operator use and not "true" for other use and not "true" for future use,

- UEs shall treat this cell as candidate during the cell selection and cell reselection procedures.

When cell broadcasts any CAG-IDs or NIDs and the cell status is indicated as "not barred" and "not reserved" for operator use and "true" for other use, and not "true" for future use:

- All NPN-capable UEs shall treat this cell as candidate during the cell selection and cell reselection procedures, other UEs shall treat this cell as if cell status is "barred".

When cell status is indicated as "true" for other use, and either cell does not broadcast any CAG-IDs or NIDs or does not broadcast any CAG-IDs and the UE is not operating in SNPN Access Mode,

- The UE shall treat this cell as if cell status is "barred".

When cell status is indicated as "true" for future use,

- The UE shall treat this cell as if cell status is "barred".

When *cellBarredNES* is absent and *cellBarred* is set to"barred",

- The UE indicating any of the values in *nes-CellDTX-DRX* shall treat this cell as if cell status is "barred".

When *cellBarredNTN* is not broadcast in this cell,

- For NTN access, the UE shall treat this cell as if cell status is "barred".

When *halfDuplexRedCapAllowed* is not broadcast in this cell,

- The (e)RedCap UE only capable of operating in half-duplex for FDD shall treat this cell as if cell status is "barred".

When *cellBarredATG* is not broadcast in this cell,

- For ATG access, the UE shall treat this cell as if cell status is "barred".

When *cellBarredFixedVSAT* is not broadcast in this cell,

- For NTN access, the fixed VSAT UE shall treat this cell as if cell status is "barred".

When *cellBarredMobileVSAT* is not broadcast in this cell,

- For NTN access, the mobile VSAT UE shall treat this cell as if cell status is "barred".

When *cellBarred2RxXR* is broadcast in this cell,

- The 2Rx XR UE shall treat this cell as if cell status is "barred".

When *intraFreqReselectionRedCap* is not broadcast in this cell,

- The RedCap UE shall treat this cell as if cell status is "barred".

When *intraFreqReselection-eRedCap* is not broadcast in this cell,

- The eRedCap UE shall treat this cell as if cell status is "barred".

When *cellBarredRedCap1Rx* is set to "barred" and *barringExemptEmergencyCall* is present in *SIB1*, if the cell will not be treated as barred by the UE for any reason other than the *cellBarredRedCap1Rx* being set to "barred" (see TS 38.331 [3]), and cell selection criteria are fulfilled as defined in clause 5.2.3,

- The RedCap UE that supports barring exemption for emergency call (see TS 38.306 [24]) and only 1Rx branch shall treat this cell as an acceptable cell.

When *cellBarredRedCap2Rx* is set to "barred" and *barringExemptEmergencyCall* is present in *SIB1*, if the cell will not be treated as barred by the UE for any reason other than the *cellBarredRedCap2Rx* being set to "barred" (see TS 38.331 [3]), and cell selection criteria are fulfilled as defined in clause 5.2.3,

- The RedCap UE that supports barring exemption for emergency call (see TS 38.306 [24]) and 2Rx branches shall treat this cell as an acceptable cell.

When *cellBarred-eRedCap1Rx* is set to "barred" and *barringExemptEmergencyCall* is present in *SIB1*, if the cell will not be treated as barred by the UE for any reason other than the *cellBarred-eRedCap1Rx* being set to "barred" (see TS 38.331 [3]), and cell selection criteria are fulfilled as defined in clause 5.2.3,

- The eRedCap UE that supports barring exemption for emergency call (see TS 38.306 [24]) and only 1Rx branch shall treat this cell as an acceptable cell.

When *cellBarred-eRedCap2Rx* is set to "barred" and *barringExemptEmergencyCall* is present in *SIB1*, if the cell will not be treated as barred by the UE for any reason other than the *cellBarred-eRedCap2Rx* being set to "barred" (see TS 38.331 [3]), and cell selection criteria are fulfilled as defined in clause 5.2.3,

- The eRedCap UE that supports barring exemption for emergency call (see TS 38.306 [24]) and 2Rx branches shall treat this cell as an acceptable cell.

When *cellBarred2RxXR* and *barringExemptEmergencyCall* are both present in *SIB1*, if the cell will not be treated as barred by the UE for any reason other than the *cellBarred2RxXR* being present in *SIB1* (see TS 38.331 [3]), and cell selection criteria are fulfilled as defined in clause 5.2.3,

- The 2Rx XR UE that supports barring exemption for emergency call (see TS 38.306 [24]) shall treat this cell as an acceptable cell.

When cell status is indicated as "not barred" and "reserved" for operator use for any PLMN/SNPN and not "true" for other use and not "true" for future use,

- UEs assigned to Access Identity 11 or 15 operating in their HPLMN/EHPLMN shall treat this cell as candidate during the cell selection and reselection procedures if the field *cellReservedForOperatorUse* for that PLMN set to "reserved".

- UEs assigned to Access Identity 11 or 15 shall treat this cell as candidate during the cell selection and reselection procedures if the field *cellReservedForOperatorUse* for selected/registered SNPN is set to "reserved".

- UEs assigned to an Access Identity 0, 1, 2 and 12 to 14 shall behave as if the cell status is "barred" in case the cell is "reserved for operator use" for the registered PLMN/SNPN or the selected PLMN/SNPN.

- UEs assigned to Access Identity 3 shall behave as if the cell status is "barred" in case the cell is "reserved for operator use" for the registered PLMN or the selected PLMN.

NOTE 1: Access Identities 11, 15 are only valid for use in the HPLMN/ EHPLMN and registered/selected SNPN; Access Identities 12, 13, 14 are only valid for use in the home country and registered/selected SNPN as specified in TS 22.261 [12].

NOTE 1a: Access Identity 3 is only valid for PLMNs that indicate to potential Disaster Inbound Roamers that the UEs can access the PLMN as specified in TS 22.261 [12].

When cell status "barred" is indicated or to be treated as if the cell status is "barred",

- The UE is not permitted to select/reselect this cell, not even for emergency calls;

- The UE shall select another cell according to the following rule:

- If the cell is to be treated as if the cell status is "barred" due to being unable to acquire the *MIB*:

- the UE may exclude the barred cell as a candidate for cell selection/reselection for up to 300 seconds.

- the UE may select another cell on the same frequency if the selection criteria are fulfilled.

- else:

- If the UE is a RedCap UE, the UE shall acquire *SIB1* and, in the remainder of this procedure, consider '*intraFreqReselection* in MIB' to be '*intraFreqReselectionRedCap* in *SIB1*', if available; or,

- If the UE is an eRedCap UE, the UE shall acquire *SIB1* and, in the remainder of this procedure, consider '*intraFreqReselection* in MIB' to be '*intraFreqReselection-eRedCap* in *SIB1*', if available; or,

- If the UE is a 2Rx XR UE, the UE shall acquire *SIB1* and, in the remainder of this procedure, consider '*intraFreqReselection* in MIB' to be '*intraFreqReselection2RxXR* in *SIB1*', if available:

- If the cell is to be treated as if the cell status is "barred" due to being unable to acquire the *SIB1*:

- the UE may exclude the barred cell as a candidate for cell selection/reselection for up to 300 seconds.

- the UE may select another cell on the same frequency if the selection criteria are fulfilled.

- If the cell status "barred" is indicated in *MIB* but the UE is unable to acquire the *SIB1*; or

- If the UE is a RedCap UE and *intraFreqReselectionRedCap* in *SIB1* is not available; or

- If the UE is an eRedCap UE and *intraFreqReselection-eRedCap* in *SIB1* is not available:

- the UE shall exclude the barred cell as a candidate for cell selection/reselection for 300 seconds.

- the UE may select another cell on the same frequency if re-selection criteria are fulfilled.

- If the UE is neither a RedCap UE nor an eRedCap UE; or

- if the UE is a RedCap UE and *intraFreqReselectionRedCap* in *SIB1* is available; or

- if the UE is an eRedCap UE and *intraFreqReselection-eRedCap* in *SIB1* is available:

- If the field *intraFreqReselection* in *MIB* message is set to "allowed":

- the UE may select another cell on the same frequency if re-selection criteria are fulfilled;

- If the cell is to be treated as if the cell status is "barred" due to no available *SIB1* request configuration for the UE supporting OD-SIB1 as defined in section 5.2.2.3.1 of TS 38.331 [3]; or

- If the cell is to be treated as if the cell status is "barred" due to maximum number of PRACH attempts is reached for the UE supporting OD-SIB1 as defined in section 5.2.2.3.3x of TS 38.331 [3]; or

- If the cell is to be treated as if the cell status is "barred" due to failing to acquire the *SIB1* upon the expiry of the *SIB1* monitoring window as defined in [4] for the UE supporting OD-SIB1; or

- If the cell is to be treated as if the cell status is "barred" due to being unable to acquire the *SIB1*:

- the UE may exclude the barred cell as a candidate for cell selection/reselection for up to 300 seconds;

- else:

- the UE shall exclude the barred cell as a candidate for cell selection/reselection for 300 seconds.

- If the field *intraFreqReselection* in *MIB* message is set to "not allowed":

- If the cell is to be treated as if the cell status is "barred" due to no available *SIB1* request configuration for the UE supporting OD-SIB1 as defined in section 5.2.2.3.1 of TS 38.331 [3]; or

- If the cell is to be treated as if the cell status is "barred" due to maximum number of PRACH attempts is reached for the UE supporting OD-SIB1 as defined in section 5.2.2.3.3x of TS 38.331 [3]; or

- If the cell is to be treated as if the cell status is "barred" due to failing to acquire the *SIB1* upon the expiry of the *SIB1* monitoring window as defined in [4] for the UE supporting OD-SIB1; or

- If the cell is to be treated as if the cell status is "barred" due to being unable to acquire the *SIB1*:

- the UE may exclude the barred cell as a candidate for cell selection/reselection for up to 300 seconds;

- If the cell operates in licensed spectrum:

- the UE shall not re-select to another cell on the same frequency as the barred cell and exclude such cell(s) as candidate(s) for cell selection/reselection for 300 seconds;

- else:

- the UE may select to another cell on the same frequency if the reselection criteria are fulfilled.

- else:

- If the cell operates in licensed spectrum, or if this cell belongs to a PLMN which is indicated as being equivalent to the registered PLMN or the selected PLMN of the UE, or if this cell belongs to an SNPN which is equal to or indicated as being equivalent to the registered SNPN or the selected SNPN of the UE:

- the UE shall not re-select to another cell on the same frequency as the barred cell and exclude such cell(s) as candidate(s) for cell selection/reselection for 300 seconds;

- else:

- the UE may select to another cell on the same frequency if the reselection criteria are fulfilled.

- the UE shall exclude the barred cell as a candidate for cell selection/reselection for 300 seconds.

The cell selection of another cell may also include a change of RAT.

If a UE supporting OD-SIB1 barred a cell due to no available *SIB1* request configuration as defined in section 5.2.2.3.1 of TS 38.331 [3], it considers the cell is no longer barred once *SIB1* request configuration of the cell is acquired.

NOTE 2: If barring of a cell is triggered by the condition of *trackingAreaCode* and *trackingAreaList* not being provided, as specified in TS 38.331 [3], the barring only applies to this PLMN and the UE can re-evaluate the barring condition again due to selection of another PLMN.

Next change

## 7.1 Discontinuous Reception for paging

The UE may use Discontinuous Reception (DRX) in RRC\_IDLE and RRC\_INACTIVE state in order to reduce power consumption. The UE monitors one paging occasion (PO) per DRX cycle. A PO is a set of PDCCH monitoring occasions and can consist of multiple time slots (e.g. subframe or OFDM symbol) where paging DCI can be sent (TS 38.213 [4]). One Paging Frame (PF) is one Radio Frame and may contain one or multiple PO(s) or starting point of a PO. A L2 U2N Relay UE monitors the paging occasions of its PC5-RRC connected L2 U2N Remote UEs. In this case, the DRX cycle and UE ID mentioned in this clause refer to those of the L2 U2N Remote UE.

In multi-beam operations, the UE assumes that the same paging message and the same Short Message are repeated in all transmitted beams and thus the selection of the beam(s) for the reception of the paging message and Short Message is up to UE implementation. The paging message is same for both RAN initiated paging and CN initiated paging.

The UE initiates RRC Connection Resume procedure upon receiving RAN initiated paging. If the UE receives a CN initiated paging in RRC\_INACTIVE state, the UE moves to RRC\_IDLE and informs NAS. However, if a L2 U2N Relay UE in RRC\_INACTIVE state receives a CN initiated paging for a L2 U2N Remote UE, the L2 U2N Relay UE does not move to RRC\_IDLE state.

NOTE 0a: The L2 U2N Remote UE does not need to monitor the PO in order to receive the paging message.

NOTE 0b: While the SDT procedure is ongoing in RRC\_INACTIVE state, the UE monitors the PO in order to receive only the Short Message as specified in TS 38.331 [3].

The PF and PO for paging are determined by the following formulae:

SFN for the PF is determined by:

(SFN + PF\_offset) mod T = (T div N)\*(UE\_ID mod N)

Index (i\_s), indicating the index of the PO is determined by:

i\_s = floor (UE\_ID/N) mod Ns

The PDCCH monitoring occasions for paging are determined according to *pagingSearchSpace* as specified in TS 38.213 [4] and *firstPDCCH-MonitoringOccasionOfPO* (or *firstPDCCH-MonitoringOccasionOfPO-r19* for paging adaptation) and *nrofPDCCH-MonitoringOccasionPerSSB-InPO* ifconfigured as specified in TS 38.331 [3]. When *SearchSpaceId* = 0 is configured for *pagingSearchSpace*, the PDCCH monitoring occasions for paging are same as for RMSI as defined in clause 13 in TS 38.213 [4].

When *SearchSpaceId* = 0 is configured for *pagingSearchSpace*, Ns is either 1 or 2. For Ns = 1, there is only one PO which starts from the first PDCCH monitoring occasion for paging in the PF. For Ns = 2, PO is either in the first half frame (i\_s = 0) or the second half frame (i\_s = 1) of the PF.

When *SearchSpaceId* other than 0 is configured for *pagingSearchSpace,* the UE monitors the (i\_s + 1)th PO. A PO is a set of 'S\*X ' consecutive PDCCH monitoring occasions where 'S' is the number of actual transmitted SSBs determined according to *ssb-PositionsInBurst* in *SIB1* and X is the *nrofPDCCH-MonitoringOccasionPerSSB-InPO* if configured or is equal to 1 otherwise. The [x\*S+K]th PDCCH monitoring occasion for paging in the PO corresponds to the Kth transmitted SSB, where x=0,1,…,X-1, K=1,2,…,S. The PDCCH monitoring occasions for paging which do not overlap with UL symbols (determined according to *tdd-UL-DL-ConfigurationCommon*) are sequentially numbered from zero starting from the first PDCCH monitoring occasion for paging in the PF. When *firstPDCCH-MonitoringOccasionOfPO* (or *firstPDCCH-MonitoringOccasionOfPO-r19* for paging adaptation) is present, the starting PDCCH monitoring occasion number of (i\_s + 1)th PO is the (i\_s + 1)th value of the *firstPDCCH-MonitoringOccasionOfPO* (or *firstPDCCH-MonitoringOccasionOfPO-r19* for paging adaptation) parameter; otherwise, it is equal to i\_s \* S\*X. If X > 1, when the UE detects a PDCCH transmission addressed to P-RNTI within its PO, the UE is not required to monitor the subsequent PDCCH monitoring occasions for this PO.

NOTE 1: A PO associated with a PF may start in the PF or after the PF.

NOTE 2: The PDCCH monitoring occasions for a PO can span multiple radio frames. When *SearchSpaceId* other than 0 is configured for *paging-SearchSpace* the PDCCH monitoring occasions for a PO can span multiple periods of the paging search space.

The following parameters are used for the calculation of PF and i\_s above:

T: DRX cycle of the UE.

If the UE does not operate in eDRX as defined in clause 7.4:

- T is determined by the shortest of the UE specific DRX value configured by RRC (if any), the UE specific DRX value configured by upper layers (if any), and a default DRX value broadcast in system information. For L2 U2N Relay UE, T for a L2 U2N Remote UE is determined by the shortest of the UE specific DRX value provided in PC5-RRC signalling and a default DRX value broadcast in system information.

In RRC\_IDLE state, if the UE operates in eDRX and eDRX is configured by upper layers, i.e., TeDRX, CN, according to clause 7.4:

- If TeDRX, CN is no longer than 1024 radio frames:

- T = TeDRX, CN;

- else:

- During CN configured PTW, T is determined by the shortest of UE specific DRX value, if configured by upper layers, and the default DRX value broadcast in system information.

In RRC\_INACTIVE state, if the UE operates in eDRX and eDRX is configured by RRC, i.e., TeDRX, RAN (if any), and upper layers, i.e., TeDRX, CN, as defined in clause 7.4:

- If both TeDRX, CN and used TeDRX, RAN are no longer than 1024 radio frames:

- T = min{TeDRX, RAN, TeDRX, CN}.

- If TeDRX, CN is no longer than 1024 radio frames and no TeDRX, RAN is configured or used:

- T is determined by the shortest of UE specific DRX value configured by RRC and TeDRX, CN.

- If TeDRX, CN is longer than 1024 radio frames:

- If TeDRX, RAN is not configured or used:

- During CN configured PTW, T is determined by the shortest of the UE specific DRX value configured by RRC, the UE specific DRX value configured by upper layers (if any), and a default DRX value broadcast in system information. Outside the CN configured PTW, T is determined by the UE specific DRX value configured by RRC;

- else if used TeDRX, RAN is no longer than 1024 radio frames:

- During CN configured PTW, T is determined by the shortest of the UE specific DRX value, if configured by upper layers and TeDRX, RAN, and a default DRX value broadcast in system information. Outside the CN configured PTW, T is determined by TeDRX, RAN;

- else if used TeDRX, RAN is longer than 1024 radio frames:

- During the overlapped part of CN configured PTW and RAN configured PTW, T is determined by the shortest of the UE specific DRX value configured by RRC, the UE specific DRX value configured by upper layers (if any), and a default DRX value broadcast in system information;

- During CN configured PTW and outside RAN configured PTW, T is determined by the shortest of the UE specific DRX value configured by upper layers (if any), and a default DRX value broadcast in system information;

- Outside CN configured PTW and during RAN configured PTW, T is determined by the UE specific DRX value configured by RRC.

N: number of total paging frames in T

Ns: number of paging occasions for a PF

PF\_offset: offset used for PF determination

UE\_ID:

If the UE operates in eDRX as specified in clause 7.4:

- 5G-S-TMSI mod 4096

else:

- 5G-S-TMSI mod 1024

Parameters *Ns*, *nAndPagingFrameOffset*, *nrofPDCCH-MonitoringOccasionPerSSB-InPO*, and the length of default DRX Cycle are signaled in *SIB1*. The values of N and PF\_offset are derived from the parameter *nAndPagingFrameOffset* as defined in TS 38.331 [3]. The parameter *firstPDCCH-MonitoringOccasionOfPO* is signalled in *SIB1* for paging in the BWP configured by *initialDownlinkBWP*.For paging in a DL BWP other than the BWP configured by *initialDownlinkBWP*, the parameter *first-PDCCH-MonitoringOccasionOfPO* is signaled in the corresponding BWP configuration.

For a UE in RRC\_IDLE or RRC\_INACTIVE state and supporting paging adaptation, if *pagingAdaptation-NS* and *pagingAdaptationNAndPagingFrameOffset* are signaled in *SIB1*, the UE determines the value of Ns from *pagingAdaptation-NS,* N and PF\_offset from the parameter *pagingAdaptationNAndPagingFrameOffset* as defined in TS 38.331 [3], and only monitors the PO(s) derived from these paging parameters. The parameter *firstPDCCH-MonitoringOccasionOfPO-r19* for paging adaptation is signalled in *SIB1* for paging in the BWP configured by *initialDownlinkBWP*. For paging in a DL BWP other than the BWP configured by *initialDownlinkBWP*, the parameter *firstPDCCH-MonitoringOccasionOfPO-r19* for paging adaptation is signaled in the corresponding BWP configuration.

If the UE has no 5G-S-TMSI, for instance when the UE has not yet registered onto the network, the UE shall use as default identity UE\_ID = 0 in the PF and i\_s formulas above.

5G-S-TMSI is a 48 bit long bit string as defined in TS 23.501 [10]. 5G-S-TMSI shall in the formulae above be interpreted as a binary number where the left most bit represents the most significant bit.

In RRC\_INACTIVE state, if the UE supports *inactiveStatePO-Determination* and the network broadcasts *ranPagingInIdlePO* with value "true", the UE shall use the same i\_s as for RRC\_IDLE state. Otherwise, the UE determines the i\_s based on the parameters and formula above.

In RRC\_INACTIVE state, if used eDRX value configured by upper layers is no longer than 1024 radio frames, the UE shall use the same i\_s as for RRC\_IDLE state.

In RRC\_INACTIVE state, if used eDRX value configured by upper layers is longer than 1024 radio frames, during CN PTW, the UE shall use the same i\_s as for RRC\_IDLE state. Outside CN PTW, the UE shall use the i\_s for RRC\_INACTIVE state.

Next change

### 7.2.1 Paging Early Indication reception

The UE may use Paging Early Indication (PEI) in RRC\_IDLE and RRC\_INACTIVE states in order to reduce power consumption. If PEI configuration is provided in system information, the UE in RRC\_IDLE or RRC\_INACTIVE state supporting PEI (except for the UEs expecting MBS group notification) can monitor PEI using PEI parameters in system information according to the procedure described below.

If *lastUsedCellOnly* is configured in system information of a cell, the UE monitors PEI in this cell only if the UE most recently received *RRCRelease* without *noLastCellUpdate* in this cell. Otherwise (i.e., if *lastUsedCellOnly* is not configured in system information of a cell), the UE monitors PEI in the camped cell.

The UE monitors one PEI occasion per DRX cycle. A PEI occasion (PEI-O) is a set of PDCCH monitoring occasions (MOs) and can consist of multiple time slots (e.g. subframes or OFDM symbols) where PEI can be sent (TS 38.213 [4]). In multi-beam operations, the UE assumes that the same PEI is repeated in all transmitted beams and thus the selection of the beam(s) for the reception of the PEI is up to UE implementation.

The time location of PEI-O for UE's PO is determined by a reference point and an offset:

- The reference point is the start of a reference frame determined by a frame-level offset from the start of the first PF of the PF(s) associated with the PEI-O, provided by *pei-FrameOffset* in SIB1;

- The offset is a symbol-level offset from the reference point to the start of the first PDCCH MO of this PEI-O, provided by *firstPDCCH-MonitoringOccasionOfPEI-O* in SIB1.

If one PEI-O is associated with POs of two PFs, the two PFs are consecutive PFs calculated by the parameters *PF\_offset*, *T*, *Ns*, and *N*. The first PF of the PFs associated with the PEI-O is provided by (SFN for PF) - floor (*iPO*/*Ns*)\**T*/*N*, where SFN for PF is determined in clause 7.1, *iPO* is defined in clause 10.4a in TS 38.213[4], *T*, *Ns*, and *N* are determined in clause 7.1.

The PDCCH MOs for PEI are determined as specified in TS 38.213 [4] according to *pei-SearchSpace*, *pei-FrameOffset*, *firstPDCCH-MonitoringOccasionOfPEI-O* and *nrofPDCCH-MonitoringOccasionPerSSB-InPO* ifconfigured as specified in TS 38.331 [3]. When *SearchSpaceId* = 0 is configured for *pei-SearchSpace*, the PDCCH MOs for PEI are same as for RMSI as defined in clause 13 in TS 38.213 [4]. UE determines first PDCCH MO for PEI-O based on *pei-FrameOffset* and *firstPDCCH-MonitoringOccasionOfPEI-O*, as for the case with *SearchSpaceId* > 0 configured.

When *SearchSpaceId* = 0 is configured for *pei-SearchSpace*, the UE monitors the PEI-O according to *searchSpaceZero*. When *SearchSpaceId* other than 0 is configured for *pei-SearchSpace,* the UE monitors the PEI-O according to the search space with the configured *SearchSpaceId*.

A PEI occasion is a set of 'S\*X' consecutive PDCCH MOs, where 'S' is the number of actual transmitted SSBs determined according to *ssb-PositionsInBurst* in *SIB1*, and X is the *nrofPDCCH-MonitoringOccasionPerSSB-InPO* if configured or is equal to 1 otherwise. The [x\*S+K]thPDCCH MO for PEI in the PEI-O corresponds to the Kth transmitted SSB, where x=0,1,…,X-1, K=1,2,…,S. The PDCCH MOs for PEI which do not overlap with UL symbols (determined according to *tdd-UL-DL-ConfigurationCommon*) are sequentially numbered from zero starting from the first PDCCH MO for PEI in the PEI-O. When the UE detects a PEI within its PEI-O, the UE is not required to monitor the subsequent MO(s) associated with the same PEI-O.

If the UE detects PEI and the PEI indicates the subgroup the UE belongs to monitor its associated PO, as specified in clause 10.4a in TS 38.213 [4], the UE monitors the associated PO as specified in clause 7.1. If the UE does not detect PEI on the monitored PEI occasion or the PEI does not indicate the subgroup the UE belongs to monitor its associated PO, as specified in clause 10.4a in TS 38.213 [4], the UE is not required to monitor the associated PO as specified in clause 7.1.

If the UE is unable to monitor the PEI occasion (i.e. all valid PDCCH MO for PEI) corresponding to its PO, e.g. during cell re-selection, the UE monitors the associated PO according to clause 7.1.

In RRC\_INACTIVE state, when the UE uses the same i­\_sas for RRC\_IDLE state as specified in clause 7.1, the UE shall use the same *iPO* as for RRC\_IDLE state. Otherwise, the UE determines the *iPO* based on the formula defined in clause 10.4a in TS 38.213 [4].

For a UE supporting paging adaptation and PEI, if *pagingAdaptationPEI-Config* is signaled in system information, the UE in RRC\_IDLE or RRC\_INACTIVE state can monitor the PEI occasion according to *pagingAdaptationPEI-Config, pei-FrameOffset-r19* and *firstPDCCH-MonitoringOccasionOfPEI-O-r19.*

End of change