**3GPP TSG-RAN WG2 Meeting #131bis R2-250xxxx**

**Prague, Czech Republic, Oct. 13-17, 2025**

**Agenda item: 8.11.1**

**Source: Samsung**

**Title: List of Rel-19 SBFD MAC open issues for maintenance**

**Document for: Discussion and Decision**

# Introduction

This offline discussion aims to collect and summarize Rel-19 SBFD MAC open issues/suggested resolutions for maintenance, compared to the agreed Rel-19 SBFD MAC CR [1], according to the instructions from Chairlady captured below.





As the result of this discussion, the Rapporteur will provide a summary outlining:

- the issues (if any) requiring further discussion with tdoc contributions in RAN2#131bis, and

- the non-controversial/editorial issues (if any) that will be handled by Rapporteur CR in RAN2#131bis, as well as the draft Rapporteur CR for review before submission deadline.

Kindly provide your input for this discussion, no later than **~~Sep. 19, 10:00 UTC~~** **Sep. 26 10:00 UTC**.

Please provide your contact information in the table below when responding.

|  |  |  |
| --- | --- | --- |
| **Company** | **Name** | **Email** |
| ZTE | Yu Pan | pan.yu24@zte.com.cn |
| Ericsson | Min Wang | Min.w.wang@ericsson.com |
| Interdigital | Jongwoo Hong | Jongwoo.hong@interdigital.com |
| Qualcomm | Ruiming Zheng | rzheng@qti.qualcomm.com |
| vivo | Dongdong Wei | weidongdong@vivo.com |
| LGE | Hanseul Hong | hanseul.hong@lge.com |
| Huawei, HiSilicon | Tao Cai | tao.cai@huawei.com |

# Co-existence of SBFD and intra-DU LTM

We have agreed to support the coexistence of SBFD and intra-DU LTM in the last meeting [2], as captured below.

|  |
| --- |
| Email discussion summary  R2-2505364 Summary of [Post130][216][SBFD] Running CR for 38.331 Huawei, HiSilicon discussion Rel-19 NR\_duplex\_evo-Core   * Noted   *[Proposals for easy agreement]:*  *[Proposal for RRC-2] Not to support that a further different SSB RSRP threshold is indicated/configured for an SSB or a group of SSBs. [13/13]*  *[Proposal for RRC-3] Not to pursue the further optimization of parameter signalling of SBFD RACH configuration. [11/12]*  *[Proposal for RRC-6] (Only) support RACH-based LTM cell change in SBFD symbols [10/11]. Add RO type indication in LTM cell switch command MAC CE.*  *[Proposals for discussion]:*  *[Proposal for RRC-1] For the network indicating RO type, use 1 bit signalling (as in the current RRC running CR) [9/13].*   * Not to support that a further different SSB RSRP threshold is indicated/configured for an SSB or a group of SSBs. * Not to pursue the further optimization of parameter signalling of SBFD RACH configuration.   Discussions  RRC-6  - Samsung object this proposal. Samsung think this should be discussed in LTM session.  - InterDigital think there is majority so we can agree, think we can discuss in SBFD because it is co-existence with Rel-18 LTM. Nokia, LG E, ZTE, CATT agree.  - ZTE think at least for intra-DU case we should be able to agree. QC agree with ZTE, think if we cannot conclude here it is not easy to agree in LTM session either. Ericsson, CATT agree.  - Samsung also has concern because there is RAN3 impact, and it is the last meeting for the WI. ZTE think if we focus on intra-DU, then there is not additional R3 impact.  - Samsung wonder if we agree which WI should handle the necessary MAC spec change.   * Support co-existence of SBFD with intra-DU LTM. Whether to support the co-existence between SBFD and other LTM cases is not discussed in the Rel-19 SBFD WI. |

***Question: Do companies think additional MAC spec change(s) compared to the agreed MAC CR [1] is needed for supporting the co-existence of SBFD and intra-DU LTM? Please provide the suggested change(s) if any.***

|  |  |  |
| --- | --- | --- |
| **Company** | **Any change is needed? (Yes/No)** | **Suggested change(s), if any** |
| ZTE | Yes | If SBFD RO can be used when UE performs intra-DU LTM, source cell should include the RO type indicator of LTM CFRA resource in both Rel-18 LTM Cell Switch Command MAC CE and Rel-19 Enhanced LTM Cell Switch Command MAC CE.  Intra-DU LTM can use both MAC CEs, if security key needs update, source cell will send Rel-19 MAC CE; if security key does not need update, source cell will send Rel-18 MAC CE.  BTW, for the above spec change, there is no additional RAN3 spec impact |
| Ericsson | Yes or No | We are fine with either way, with the changes proposed by ZTE, LTM can be better supported with SBFD, without the changes, it is also workable, i.e., UE relies on dedicated RRC signaling to derive RO type. |
| IDC | Yes | Since RAN2 agreed to support co-existence of SBFD with intra-DU LTM, this agreement should be captured/specified in MAC spec.  As ZTE mentioned, RO type indication can be included in the Rel-18 and Rel-19 LTM cell switch MAC CE (e.g., intra-DU LTM case) |
| Qualcomm | Yes | RO type indication can be included in the Rel-18 and Rel-19 LTM cell switch MAC CE in Rel-19 MAC specification. |
| vivo | Yes | Share the same view as ZTE. |
| LGE | Yes, slightly | In our understanding, if the RO type can be indicated via RRC signalling (i.e., RO type indication via RACH-ConfigDedicated IE) for LTM cell switch, it could also be indicated by the LTM cell switch MAC CE with similar reason.  For RAN3 impact, aligned with ZTE, i.e., there is no additional RAN3 impact for indicating RO type in LTM Cell switch MAC CE. |
| Huawei, HiSilicon | Yes with comments | The understanding during online session was to use a separate CR (not MAC running CR) to add RO type indicator in Rel-19 LTM cell change command MAC CE and it was assumed not to change Rel-18 MAC CE (contrary to what was proposed in the pre RAN2#131 RRC open issue discussion summary). Calling it Rel-18 MAC CE in a Rel-19 CR/spec seems odd, however we are fine if majority thinks Rel-18 MAC CE is to be used when security key does not need update as in ZTE comments. |

**Rapp summary**: The discussion on this issue has shown that companies are largely aligned that, to support coexistence of SBFD and intra-DU LTM, RO type signalling should be integrated into both Rel-18 and Rel-19 LTM cell switch command MAC CEs.

**Proposed WF**: Given the non-controversial resolution for this issue, as per the Chairlady's instruction, the Rapporteur CR will incorporate the RO type signalling/selection for the cases of Rel-18 and Rel-19 LTM cell switch command MAC CEs. A draft CR will be shared soon for companies to review before submission deadline.

# Other MAC open issues for maintenance

Please share any other identified MAC open issues for maintenance, by explaining what the issue is, and the suggested change(s), including editorial improvement. Note that, as the WI has been declared complete, the Rapporteur will not consider the issue(s) involving any further functional changes, for further discussion.

|  |  |  |  |
| --- | --- | --- | --- |
| **Company** | **Identified issues** | **Suggested change(s)** | **Rapp comment** |
| Ericsson | *sbfd-RO-Type is not included in the parameter list in clause 5.1.1* | Include *sbfd-RO-Type in the parameter list* | Agree and thanks for thorough review. Will be incorporated in Rapp CR. |
| Ericsson | 1> if the *RO\_TYPE* is set to *2nd-RO*:  2> set the *RA\_TYPE* to *4-stepRA*.  The above condition highlighted in yellow is not needed/wrong.  The logic is that: it can be up to gNB configuration to ensure that 2-step RA and SBFD will not be present in the same cell/BWP. | There may be several options to address the scenario, where the SBFD aware UE is configured with both 2-step RA and SBFD  Option 1 – up to gNB configuration to ensure that 2-step RA and SBFD will not be present in the same cell/BWP.  RAN2 can further check if some restriction text is needed in RRC.  Option 2 – UE has 2-step RA and SBFD RO selected, UE falls back to 4-step RA (as captured in the rapporteur CR)  Option 3 – UE has 2-step RA and SBFD RO selected, UE falls back to legacy RO. | An offline discussion (3.1) is triggered below for this issue.  Note that Option 3 is precluded for further discussion, given that it is a new UE behavior that is out of the maintenance scope.  Ericsson-> we don’t agree with that option 3 is a new UE behavior.  The issue itself is not discussed in RAN2 yet, the implemented Option 2 is just an artificial implementation by RAPP, there is no RAN2 agreement.  If you want companies to discuss the issue, it is more correct to list all options.  **[Rapp reply]** I understand your concern is lack of formal agreement on the prioritization between RA type selection and RO type selection. But, you know, we have already concluded RO type selection is performed in the very beginning prior to other steps, based on which, the CR and the past several open issue discussions have been conducted.  For your reference, I added my explanation why I deemed option 3 as new UE behavior below. If you think I mis-understood your intention, please provide the proposed TP in the suggested changes, for (at least) me and other companies to fully understand it. Otherwise, I can't let companies make decision without a clear understanding on its impact on UE behavior and the specification.  **[Rapp explanation]** Considering the three steps that UE has to perform sequentially, with inter-dependencies between consecutive steps, i.e., [step 1] RO type selection => [step 2] RACH resource set selection (based on the selected RO type) => [step 3] RA type selection (based on the selected RACH resource set), my understanding of your option 3 is to allow UE that has selected SBFD RO (in [step 1]) and 2-step RA (in [step 3]), to fallback to legacy RO. But please note that the consequence would be, UE needs to re-select RACH resource set for legacy RO (note that in RACH config option 2, RACH resource set of SBFD RO and legacy RO are provided separately), and then, [step 3] should be performed again, based on the re-selected RACH resource set (note that 2-step RA can be selected only when the 2-step resource is provided by the selected RACH resource set). Also, we can't even guarantee that 2-step RA will be selected again when re-doing the [step 3] with the re-selected RACH resource set, since there could be no 2-step RA resource provided by the re-selected RACH resource set for legacy RO, such that we may end up with legacy RO with 4-step RA (even though SBFD RO is selected in the very beginning). From my perspective, such operation is a new type of RO type fallback that is deemed as new UE behavior. |
| LGE | As we commented during the CR review, it may be needed to be clarified that the highlighted preambleReceivedTargetPower should not be the value included in the *sbfd-RACH-DualConfig,* which is not used for initialization when the UE selects the 2nd-RO.  5> else (i.e., the received UL grant indicates that the corresponding PUSCH transmission is in non-SBFD symbols as specified in clause 11.1 of TS 38.213 [6]):  6> indicate the preambleReceivedTargetPower and the amount of power ramping applied to the latest Random Access Preamble transmission to lower layers (i.e. (PREAMBLE\_POWER\_RAMPING\_COUNTER – 1) × PREAMBLE\_POWER\_RAMPING\_STEP + POWER\_OFFSET\_2STEP\_RA + POWER\_OFFSET\_RO\_TYPE); | If the 1st RO is selected for preamble transmission but the Msg3 PUSCH is transmitted in SBFD symbol, the *preambleReceivedTargetPower* in *sbfd-RACH-DualConfig* should be used even though it is not used for initialization. It is already captured as follows:   |  | | --- | | 6> else if sbfd-RACH-DualConfig (see TS 38.331 [5]) is configured for the Random Access procedure:  7> indicate the preambleReceivedTargetPower included in the sbfd-RACH-DualConfig, and the amount of power ramping applied to the latest Random Access Preamble transmission to lower layers (i.e. (PREAMBLE\_POWER\_RAMPING\_COUNTER – 1) × PREAMBLE\_POWER\_RAMPING\_STEP + POWER\_OFFSET\_2STEP\_RA + POWER\_OFFSET\_RO\_TYPE). |   Therefore, for the mentioned case, similar text may be used, e.g.,   |  | | --- | | 5> else (i.e., the received UL grant indicates that the corresponding PUSCH transmission is in non-SBFD symbols as specified in clause 11.1 of TS 38.213 [6]):  6> indicate the preambleReceivedTargetPower (not included in sbfd-RACH-DualConfig) and the amount of power ramping applied to the latest Random Access Preamble transmission to lower layers (i.e. (PREAMBLE\_POWER\_RAMPING\_COUNTER – 1) × PREAMBLE\_POWER\_RAMPING\_STEP + POWER\_OFFSET\_2STEP\_RA + POWER\_OFFSET\_RO\_TYPE); | | An offline discussion (3.2) is triggered for this issue below. |

**Rapp summary**: From the Rapporteur's perspective, two additional issues worth further offline discussions, have been identified based on the inputs from companies. Consequently, the discussions seeking companies' views are triggered below, respectively, to determine whether tdoc contributions are required for these issues for the upcoming meeting.

## RO Type and RA Type Selections

**Issue description (Ericsson)**:

|  |  |
| --- | --- |
| Given the consensus that SBFD RO is not supported for 2-step RA, and the RO type selection is performed before RA type selection, there are largely two options in implementing the expected UE behaviour, i.e., UE selecting SBFD RO performs 4-step RA.  **Option 1) (as specified in SBFD MAC CR [1])**  - Explicitly capturing UE behaviour for the case when RO type is set to SBFD RO, 4-step RA is selected, i.e., maintaining the RO type condition in RA selection (in yellow) captured in SBFD MAC CR [1].   |  | | --- | | *CR#R2-2506606*  5.1.1 Random Access procedure initialization  …  1> if the *RO\_TYPE* is set to *2nd-RO*:  2> set the *RA\_TYPE* to *4-stepRA*.  … |   **Option 2) (proposed by Ericsson)**  - Relying on a proper network configuration (which ensures expected UE behaviour) without explicitly capturing the relevant UE behavior in MAC spec, i.e., removing the RO type condition in RA selection captured in SBFD MAC CR [1]. |

**Discussion:**

***Question: From MAC spec point of view, for preventing UE that has selected SBFD RO, from performing 2-Step RA, which option do companies prefer?***

***- Option 1) Maintaining the RO type condition in RA selection (as specified in SBFD MAC CR [1]),***

***- Option 2) Removing the RO type condition in RA selection,***

***- Option 3) Need further discussion via tdoc contribution in RAN2#131bis.***

|  |  |  |
| --- | --- | --- |
| **Company** | **Option 1 or 2 or 3** | **Comments if any** |
| Ericsson | We are fine with either option 2 or option 3. | **Option 1 is an artificial implementation by the RAPP, there is no corresponding RAN2 agreement**  **[Rapp]** Companies may have different preference on how to model the expected UE behavior, but can't agree it is "artificially" implemented by Rapporteur, given that the change is triggered by companies' comment during CR review, and no concerns that had been shared afterwards. FYI, bubbles below are the discussion on how this change is introduced. It may be helpful also for other companies in their decision-making.   |  | | --- | | **[Post130][217][SBFD] Running CR for 38.321 (Samsung)**  [Draft\_R2-25xxxx MAC Running CR for SBFD\_v07\_Rapp (reply)](https://www.3gpp.org/ftp/Email_Discussions/RAN2/%5BRAN2%23130%5D/%5BPost130%5D%5B217%5D%5BSBFD%5D%20Running%20CR%20for%2038.321%20(Samsung)/Draft_R2-25xxxx%20MAC%20Running%20CR%20for%20SBFD_v07_Rapp%20(reply).docx)  1> if the contention-free Random Access Resources have been explicitly provided in the LTM Cell Switch Command MAC CE:  2> set the *RA\_TYPE* to *4-stepRA*.  1> else if the *RO\_TYPE* is set to *non-SBFD-RO*, and the BWP selected for Random Access procedure is configured with both 2-step and 4-step RA type Random Access Resources within the selected set of Random Access resources (as specified in clause 5.1.1b) and the RSRP of the downlink pathloss reference is above *msgA-RSRP-Threshold*; or  1> if the BWP selected for Random Access procedure is only configured with 2-step RA type Random Access resources within the selected set of Random Access resources according to clause 5.1.1b; or  1> if the Random Access procedure was initiated for reconfiguration with sync not initiated for recovery using an LTM candidate configuration as specified in TS 38.331 [5] clause 5.3.7.3 and if the contention-free Random Access Resources for 2-step RA type have been explicitly provided in *rach-ConfigDedicated* for the BWP selected for Random Access procedure:  2> set the *RA\_TYPE* to *2-stepRA*. | |
| Nokia | Option 1 | We think the current MAC CR is in good shape and helps to avoid any wrong network configuration of 2-step RACH for SBFD RO. |
|  |  |  |

**Summary:**

## *preambleReceivedTargetPower* for Msg3 Tx Power

**Issue description (LGE)**:

|  |  |  |  |
| --- | --- | --- | --- |
| According to RAN1#120bis agreement captured below,   |  | | --- | | RAN1#120bis  For determination of the Msg3 PUSCH transmission power for RACH configuration Option 2:  - preambleReceivedTargetPower configured for legacy-RO is used if Msg3 PUSCH is transmitted in non-SBFD symbols;  - preambleReceivedTargetPower configured for additional-RO is used if Msg3 PUSCH is transmitted in SBFD symbols; |   the Rapporteur captured the corresponding UE behavior in SBFD MAC CR [1] by:   |  | | --- | | *CR#R2-2506606*  5.1.4 Random Access Response reception  …  5> if the received UL grant indicates that the corresponding PUSCH transmission is in SBFD symbols as specified in clause 11.1 of TS 38.213 [6]:  6> if *sbfd-RACH-SingleConfig* (see TS 38.331 [5]) is configured for the Random Access procedure:  7> indicate the *sbfd-RACH-SingleConfig-preambleReceivedTargetPower* if configured, or the *preambleReceivedTargetPower* otherwise, and the amount of power ramping applied to the latest Random Access Preamble transmission to lower layers (i.e. (*PREAMBLE\_POWER\_RAMPING\_COUNTER* – 1) × *PREAMBLE\_POWER\_RAMPING\_STEP +* *POWER\_OFFSET\_2STEP\_RA* + *POWER\_OFFSET\_RO\_TYPE*).  6> else if *sbfd-RACH-DualConfig* (see TS 38.331 [5]) is configured for the Random Access procedure:  7> indicate the *preambleReceivedTargetPower* included **in the *sbfd-RACH-DualConfig***, and the amount of power ramping applied to the latest Random Access Preamble transmission to lower layers (i.e. (*PREAMBLE\_POWER\_RAMPING\_COUNTER* – 1) × *PREAMBLE\_POWER\_RAMPING\_STEP +* *POWER\_OFFSET\_2STEP\_RA* + *POWER\_OFFSET\_RO\_TYPE*).  6> else:  7> indicate the *preambleReceivedTargetPower* and the amount of power ramping applied to the latest Random Access Preamble transmission to lower layers (i.e. (*PREAMBLE\_POWER\_RAMPING\_COUNTER* – 1) × *PREAMBLE\_POWER\_RAMPING\_STEP +* *POWER\_OFFSET\_2STEP\_RA* + *POWER\_OFFSET\_RO\_TYPE*).  5> else (i.e., the received UL grant indicates that the corresponding PUSCH transmission is in non-SBFD symbols as specified in clause 11.1 of TS 38.213 [6]):  6> indicate the *preambleReceivedTargetPower* and the amount of power ramping applied to the latest Random Access Preamble transmission to lower layers (i.e. (*PREAMBLE\_POWER\_RAMPING\_COUNTER* – 1) × *PREAMBLE\_POWER\_RAMPING\_STEP +* *POWER\_OFFSET\_2STEP\_RA* + *POWER\_OFFSET\_RO\_TYPE*).  … |   Note that, based on the RAN1 agreement, the *preambleReceivedTargetPower* indicated to lower layer for Msg3 tx power calculation solely depends on the type of symbols (SBFD or non-SBFD) the corresponding Msg3 is transmitted in, irrespective of the RO type used in preamble transmission, and hence, is not necessarily the same parameter (re)initialized for the preamble transmission(s).  One company (LGE) shared a concern that "the *preambleReceivedTargetPower*" (without further condition) can be mis-interpreted as the one used/initialized for preamble transmission, and proposed to clarify explicitly with the condition below for avoiding such mis-interpretation, i.e.,  **[TP of LGE]**   |  | | --- | | …  5> else (i.e., the received UL grant indicates that the corresponding PUSCH transmission is in non-SBFD symbols as specified in clause 11.1 of TS 38.213 [6]):  6> indicate the *preambleReceivedTargetPower* (not included in *sbfd*-*RACH*-*DualConfig*) and the amount of power ramping applied to the latest Random Access Preamble transmission to lower layers (i.e. (*PREAMBLE\_POWER\_RAMPING\_COUNTER* – 1) × *PREAMBLE\_POWER\_RAMPING\_STEP +* *POWER\_OFFSET\_2STEP\_RA* + *POWER\_OFFSET\_RO\_TYPE*). |   The Rapporteur had also shared the similar concern when drafting the running CR that, for the same purpose, captured the parameters with distinctive texts, i.e., with and without "**in the *sbfd-RACH-DualConfig***", to differentiate the parameters configured for SBFD RO and legacy RO, respectively, for SBFD RACH config option 2. |

**Discussion:**

***Question 1: For the case that Msg3 is transmitted in non-SBFD symbols and SBFD RACH config option 2 is configured, do companies think further spec change(s) is needed, compared to the SBFD MAC CR [1], to clarify the preambleReceivedTargetPower used in Msg3 transmission power calculation is that configured for legacy RO?***

***Question 2: If so, please indicate whether to support TP of LGE or not (meaning further discussion via tdoc contribution is needed in RAN2#131bis).***

|  |  |  |  |
| --- | --- | --- | --- |
| **Company** | **Need further change (Y/N)** | **Support TP of LGE (Y/N)** | **Comments if any** |
| Ericsson | Slight prefer LGE solution | Y | With LG’s suggested changes, it can help to avoid any mis-interpretation.  We are fine with LG’s TP. |
| Nokia | Y | Y | We are ok with LG’s TP |
|  |  |  |  |
|  |  |  |  |

**Summary:**

# Conclusions

The following issues have been identified based on the discussion.

**Issues for further discussion with tdoc contributions in RAN2#131bis:**

**…**

**Issues that will be handled by Rapporteur CR for RAN2#131bis:**

**…**

# References

1. R2-2506606 , CR#2106, Samsung
2. R2-2506202 Report from session on Rel-18 MIMO, Rel-19 MIMO, LPWUS, SBFD, NR Others RAN2 Vice Chairman (CATT)