**3GPP TSG RAN WG2 Meeting #131bis R2-250xxxx**

Prague, Czech, Oct 13th – 17th, 2025

Agenda Item: 8.20.1

Source: CATT

Title: Report of [Post131][225][NR\_Others] On Rx BSF optimization (CATT)

Document for: Discussion and Decision

# Introduction

* [Post131][225][NR\_Others] On Rx BSF optimization (CATT)

Intended outcome: Discussion summary on the UAI issue, and endorse the CR for TS38.331

Deadline: Long

Rapporteur will provide RRC CR for RAN2#131bis based on the outcome of this post email discussion.

Companies providing input to this email discussion are requested to leave contact information below.

|  |  |  |
| --- | --- | --- |
| **Company** | **Name** | **Email Address** |
| vivo | Dongdong Wei | weidongdong@vivo.com |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

# Discussion

In RAN4 LS [1], the updated RAN4 agreements on Rx BSF are provided as below. And RAN2 work is to introduce a new UAI indicating UE preference to quit FBS. Regarding the UAI details, some issues have been listed and companies are invited to provide views.

|  |  |  |
| --- | --- | --- |
| 1. Overall Description:  RAN4 would like to update RAN2 on the Rx BSF optimization for NR RRM Phase 5. RAN4 had discussion on the Rx BSF optimization and the following agreements have been made for quitting condition of FBS:   |  | | --- | | RAN4#115 Agreement:  For the quitting condition of FBS:   * Introduce a new UAI indicating “overheating” issue:   + RAN4 will not discuss the UE behaviour after reporting UAI * Introduce a timer-based solution:   + UE is allowed to fall back to normal measurement when it has performed fast measurement for at least T1 from the time point when UE enters the FBS mode after meeting the FBS entry condition     - Further discuss the candidate numbers for T1. |   RAN4 further discussed the UAI and updated the agreement as follows:   * Introduce a new UAI indicating UE preference to quit FBS:   + RAN4 will not discuss the UE behaviour after reporting UAI   For the value of T1, RAN4 agreed to define a fixed a value of 90 seconds in RAN4 spec, which has no RAN2 impact in RAN4 understanding.   |  | | --- | | RAN4#116 Agreement:  A fixed value of 90 seconds. |   2. Actions:  **To RAN WG2 group:**  **ACTION:**  **RAN4 kindly requests RAN2 to take the above agreements into consideration for future work and define the new UAI in RAN2 specification.** |

***UAI Content***

The UAI is used to indicate UE preference to quit FBS, then whether the following UAI content is agreeable:

quitFBS-PreferenceFR2-r19 ENUMERATED {true} OPTIONAL

##### Q1. Do you agree the new UAI only indicates UE preference to quit FBS?

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comment** |
| vivo | Yes | Follow RAN4 agreements. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

##### Summary

***Prohibit timer***

Prohibit timer can prevent UE from frequently reporting UAI information. For example, T346m has been introduced for multi-Rx preference reporting. And the configuration of timer length is as below, i.e., timer length in seconds.

MultiRx-PreferenceReportingConfigFR2-r18 ::= SEQUENCE {

multiRx-PreferenceReportingConfigFR2ProhibitTimer-r18 ENUMERATED {

s0, s0dot5, s1, s2, s3, s4, s5, s6, s7,

s8, s9, s10, s20, s30, spare2, spare1}

}

|  |
| --- |
| ***multiRx-PreferenceReportingConfigFR2ProhibitTimer***  Prohibit timer for multi-Rx operation preference reporting for FR2. Value in seconds. Value *s0* means prohibit timer is set to 0 seconds, value *s0dot5* means prohibit timer is set to 0.5 seconds, value *s1* means prohibit timer is set to 1 second and so on. |

Considering RAN4 has agreed that:

*UE is allowed to fall back to normal measurement when it has performed fast measurement for 90s from the time point when UE enters the FBS mode after meeting the FBS entry condition.*

it seems unnecessary to introduce a prohibit timer for this new UAI, as the time duration of FBS operation is only 90s, and after receiving this quitting-preference UAI during this 90s period, network can lower down the activation threshold so that UE can quit FBS operation.

##### Q2. Do you agree NOT to introduce a prohibit timer for this new UAI?

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comment** |
| vivo | Yes | No need to introduce a duplicated timer in RAN2. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

##### Summary

***UAI configuration***

**Q3. If the answer to Q2 is Yes, whether the following configuration to enable the new UAI is agreeable:**

OtherConfig-v19xy ::= SEQUENCE {

quitFBS-PreferenceReportingConfigFR2-r19 ENUMERATED {true} OPTIONAL -- Need R

}

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comment** |
| vivo | Yes |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

***UAI procedure***

**Q4. If the answers to the questions above are all Yes, whether the following UAI related procedural text in RRC is agreeable:**

|  |
| --- |
| 5.7.4.2 Initiation  <Unnecessary part omitted>  1> if configured to provide its preference for quitting FBS operation:  2> if the UE has a preference on quitting FBS operation for FR2:  3> initiate transmission of the *UEAssistanceInformation* message in accordance with 5.7.4.3 to provide the UE preference for quitting FBS operation for FR2.  5.7.4.3 Actions related to transmission of *UEAssistanceInformation* message  <Unnecessary part omitted>  1> if transmission of the *UEAssistanceInformation* message is initiated to provide preference on quitting FBS operation for FR2 according to 5.7.4.2:  2> set *quitFBS-PreferenceFR2* to *true*: |

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comment** |
| vivo | Yes | Besides these modifications, we prefer also adding this purpose (i.e. preference on quitting FBS operation) into section 5.7.4.1, e.g.  - configured grant assistance information for NR sidelink positioning, or  - its preference on quitting FBS operation for FR2. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

##### Summary:

***Any other issues on the new UAI***

##### Q5. For any other issues companies think RAN2 needs to discuss about this new UAI, please add them in the following table.

|  |  |
| --- | --- |
| **Company** | **Comment** |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

##### Summary

***RRC CR***

##### Q6. Regarding the following RRC CR, companies are invited to leave further comments in the following table.

[R2-2505205](file:///C:\Users\panidx\OneDrive%20-%20InterDigital%20Communications,%20Inc\Documents\3GPP%20RAN\TSGR2_131\Docs\R2-2505205.zip) Introduction of Rx BSF optimization for NR RRM Ph5 CATT, Ericsson, Apple, ZTE Corporation draftCR Rel-19 38.331 18.6.0 B NR\_RRM\_Ph5-Core

|  |  |
| --- | --- |
| **Company** | **Comment** |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

##### Summary

# Conclusion

# References

[1] R4-2512333, LS on Rx BSF optimization for NR RRM Phase 5