**3GPP TSG-RAN WG2 Meeting #131 R2-250xxxx**

**Bengaluru, India, August 25th – 29th, 2025**

**Agenda Item: 8.13.1**

**Source: Huawei, HiSilicon**

**Title: Comment collection for RRC (TS 38.331) running CR for NR Sidelink Multihop Relay**

**Document for:**

# 1 Introduction

This paper collects any further comments for RRC (TS 38.331) running CR for NR Sidelink Multihop Relay

* [Post131][414][Relay] Rel-19 relay 38.331 CR (Huawei)

Scope: Update the CR in R2-2505714 in accordance with decisions of RAN2#131.

Intended outcome: Agreed CR in R2-2506326

Deadline: Short (for RP) – 4th September 12:00 UTC

Please fill in the contact information in the table below

|  |  |  |
| --- | --- | --- |
| **Company** | **Contact Person** | **Email Address** |
| CATT | Hao Xu | xuhao@catt.cn |
| OPPO | Bingxue Leng | lengbingxue@oppo.com |
|  |  |  |
|  |  |  |
|  |  |  |

# 2 Comments for the running CR

This section is used to collect comments for the Merged RRC (TS 38.331) running CR for NR Sidelink Multihop Relay

|  |  |  |
| --- | --- | --- |
| **Company** | **Issue** | **Suggestion** |
| CATT | Redundant punctuation mark at the end of the terminology for Last U2N Relay UE in 3.1. | Delete it. |
| CATT | Redundant punctuation mark at the end of 5.8.9.9.X. | Delete it. |
| CATT | In 5.8.9.10.2, there are some typos. | “ot Last U2N Relay UEs” should be changed to “or Last U2N Relay UE’s”. |
| OPPO | In clause 5.8.9.10, our understanding is we have no agreement on this condition:  2> upon reception of an *NotificationMessageSidelink* from the parent while in RRC\_CONNECTED; | Remove the related initiation condition and behaviors |
| OPPO | In clause 5.8.9.10.3, for the cause value for relay reselection and cell selection case, we understand during online session, it was said the cause value to be used can be discussed in running CR. Considering both cases are path switching but just different results, i.e., whether PC5 or Uu is available, we prefer to use a single cause value to avoid 2 new cause values for the same case. | Use a single cause value for relay reselection and cell selection, e.g., relayUE-pathSwitcing since they are same case with different results (i.e., whether cell or relay is available) |
| OPPO | The change on change should be removed (e.g., in clause 4.2.2, 5.2.2.2.1, 5.8.3.2) |  |
| OPPO | The Uu threshold needs to be checked by the intermediate relay UE for discovery transmission and SUI initiation as in legacy | In clause 5.8.3.2,  3> if the last transmission of the *SidelinkUEInformationNR* message did not include *sl-TxResourceReqListDisc*; or if the information carried by the *sl-TxResourceReqListDisc* has changed since the last transmission of the *SidelinkUEInformationNR* message:  4> if the UE is capable of U2N Relay UE or of Last U2N Relay UE, and if *SIB12* includes *sl-RelayUE-ConfigCommon*, and if the U2N Relay UE or if the Last U2N Relay UE threshold conditions as specified in 5.8.14.2 are met; or  4> if the UE is capable of Intermediate U2N Relay UE, and if SIB12 includes sl-RelayUE-ConfigCommonMH and *sl-RemoteUE-ConfigCommon*, and if the and if the U2N Remote UE threshold conditions as specified in 5.8.15.2 are met; or  In clause 5.8.13.3,  2> if the UE is in RRC\_CONNECTED and uses the frequency included in *sl-ConfigDedicatedNR* within *RRCReconfiguration* message:  3> if the UE is acting as NR sidelink U2N Relay UE or Last U2N Relay UE and *sl-DiscConfig* is included in *RRCReconfiguration*, and if the NR sidelink U2N Relay UE or Last U2N Relay UE threshold conditions as specified in 5.8.14.2 are met based on *sl-RelayUE-Config*; or3> if the UE is selecting NR sidelink U2N Relay UE / has a selected NR sidelink U2N Relay UE/ configured with measurement object associated to L2 U2N Relay UEs in both single hop or multi hop case and *sl-DiscConfig* is included in *RRCReconfiguration*, and if the NR sidelink U2N Remote UE threshold conditions as specified in 5.8.15.2 are met based on *sl-RemoteUE-Config*; or  3> if the UE acting as Last U2N Relay UE is sending Discovery Response message with Model B as specified in TS 23.304 [65] and if both the NR sidelink multi-hop relay threshold conditions as specified in 5.8.x.2 are met based on *sl-RelayUE-ConfigMH* and the NR sidelink U2N Relay UE threshold conditions as specified in 5.8.14.2 are met based on *sl-RelayUE-Config*; or  3> if the UE acting as Intermediate U2N Relay UE is sending Discovery Solicitation message with Model B as specified in TS 23.304 [65] and if both the NR sidelink multi-hop relay threshold conditions as specified in 5.8.x.2 are met based on *sl-RelayUE-ConfigMH* and the NR sidelink U2N Relay UE threshold conditions as specified in 5.8.14.2 are met based on *sl-RelayUE-Config*; or  …  2> else if the cell chosen for NR sidelink discovery transmission provides *SIB12*:  3> if the UE is acting as NR sidelink U2N Relay UE or Last U2N Relay UE and *sl-DiscConfigCommon* is included in *SIB12*, and if the NR sidelink U2N Relay UE or Last U2N Relay UE threshold conditions as specified in 5.8.14.2 are met based on *sl-RelayUE-ConfigCommon* in *SIB12*; or  3> if the UE is selecting NR sidelink U2N Relay UE / has a selected NR sidelink U2N Relay UE in both single hop or multi hop case and *sl-DiscConfigCommon* is included in *SIB12*, and if the NR sidelink U2N Remote UE threshold conditions as specified in 5.8.15.2 are met based on *sl-RemoteUE-ConfigCommon* in *SIB12*; or  3> if the UE acting as Intermediate U2N Relay UE has an established PC5 link with the selected parent U2N Relay UE, and if the NR sidelink U2N Remote UE threshold conditions as specified in 5.8.15.2 are met based on *sl-RemoteUE-ConfigCommon* in *SIB12*; or  3> if the UE acting as Intermediate U2N Relay UE is sending Discovery Solicitation message with Model B as specified in TS 23.304 [65] and *sl-DiscConfigCommon* is included in *SIB12*, and if both the NR sidelink multi-hop relay threshold conditions as specified in 5.8.x.2 are met based on *sl-RelayUE-ConfigCommonMH* and *sl-RemoteUE-ConfigCommon*, and if the and if the U2N Remote UE threshold conditions as specified in 5.8.15.2 are met; or  3> if the UE acting as Last U2N Relay UE is sending Discovery Response message with Model B as specified in TS 23.304 [65] and *sl-DiscConfigCommon* is included in *SIB12*, and if both the NR sidelink multi-hop relay threshold conditions as specified in 5.8.x.2 are met based on *sl-RelayUE-ConfigCommonMH* and the NR sidelink U2N Relay UE threshold conditions as specified in 5.8.14.2 are met based on *sl-RelayUE-Config*; or |
| OPPO | This agreement is not captured and should be added  Similar to SIB request, a paging information list is introduced for the intermediate relay UE to carry the paging information from the downstream remote UEs. Signalling details can be checked in the ASN.1 review as usual. | TP can be as follows  1> if the UE has paging related information to provide (e.g. the UE has not sent *sl-PagingInfo-RemoteUE* in the *RemoteUEInformationSidelink* message to the parent L2 U2N Relay UE before),set *sl-PagingInfo-RemoteUE/ sl-PagingInfo-RemoteUE-List* as follows:  2> if the L2 U2N Remote UE is in RRC\_IDLE:  3> include *ng-5G-S-TMSI* in the *sl-PagingIdentityRemoteUE*;  3> if the UE specific DRX cycle is configured by upper layer, set *sl-PagingCycleRemoteUE* to the value of UE specific Uu DRX cycle configured by upper layer*;*  2> else if the L2 U2N Remote UE is in RRC\_INACTIVE:  3> include *ng-5G-S-TMSI* and *fullI-RNTI* in the *sl-PagingIdentityRemoteUE*;  3> if the UE specific DRX cycle is configured by upper layer,  4> set *sl-PagingCycleRemoteUE* to the minimum value of UE specific Uu DRX cycles (configured by upper layer and configured by RRC)*;*  3> else:  4> set *sl-PagingCycleRemoteUE* to the value of UE specific DRX cycle configured by RRC;  2> if any paging informationis received from the Child UE:  3> include the received paging informationin the *sl-PagingInfo-RemoteUE-List*;  <…>  RemoteUEInformationSidelink-r17-IEs ::= SEQUENCE {  sl-RequestedSIB-List-r17 SetupRelease { SL-RequestedSIB-List-r17} OPTIONAL, -- Need M  sl-PagingInfo-RemoteUE-r17 SetupRelease { SL-PagingInfo-RemoteUE-r17} OPTIONAL, -- Need M  lateNonCriticalExtension OCTET STRING OPTIONAL,  nonCriticalExtension RemoteUEInformationSidelink-v1800-IEs OPTIONAL  }  RemoteUEInformationSidelink-v1800-IEs ::= SEQUENCE {  sl-RequestedPosSIB-List-r18 SetupRelease { SL-RequestedPosSIB-List-r18 } OPTIONAL, -- Need M  sl-SFN-DFN-OffsetRequested-r18 ENUMERATED { true } OPTIONAL, -- Need R  connectionForMP-r18 ENUMERATED {true} OPTIONAL, -- Need N  sl-DestinationIdentityRemoteUE-r18 SL-DestinationIdentity-r16 OPTIONAL, -- Need N  nonCriticalExtension RemoteUEInformationSidelink-v1900-IEs OPTIONAL  }  RemoteUEInformationSidelink-v1900-IEs ::= SEQUENCE {  sl-PagingInfo-RemoteUE-List-r19 SetupRelease { SL-PagingInfo-RemoteUE-List-r19} OPTIONAL, -- Need M  SL-PagingInfo-RemoteUE-List-r19 ::= SEQUENCE (SIZE (max)) OF SL-PagingInfo-RemoteUE-r17 |
| Samsung | Trigger of notification message in case of intermediate relay UE is in IDLE/INACTIVE state. The following agreements are not captured:  In case of notification message triggered by an error (e.g., RLF), for intermediate relay UE in idle/inactive, the intermediate relay UE can send cell/relay reselection cause value to the remote UE in RRC\_IDLE/INACTIVE if it successfully performs a recovery action. If recovery action is not successful or if it opts to release the upstream PC5 link, it sends relayUE-PC5-RLF cause value if PC5 RLF is detected by itself or the same cause value received in the notification message from the parent node. | The agreement indicates that the cause of cell/relay reselection is sent after the successful recovery of the intermediate relay UE in idle/inactive; while the cause of relayUE-PC5-RLF is sent after unsuccessful recovery or release of upstream PC5 link, or detection of PC5 RLF by itself, or same cause value is received from the parent node.  However, such agreement is not quite clear. It may need further clarification in the next meeting. |
| Samsung | Indication Type in notification message.  In indicationType-r19, only the new cause is needed. | indicationType-r19 ENUMERATED {  ~~relayUE-Uu-RLF, relayUE-HO, relayUE-CellReselection,~~  ~~relayUE-Uu-RRC-Failure,~~relayUE-RelayReselection,  relayUE-CellSelection, ~~relayUE-PC5-RLF,~~ spare1  } OPTIONAL, -- Need N |
| Sharp | In RRC connection establishment procedure, the following wording has been added:  1> if the UE is acting as L2 U2N Remote UE or is acting as L2 Intermediate U2N Relay UE: | Add the same wording for RRC re-establishment procedure and RRC resume procedure; or remove the added wording in RRC connection establishment procedure. |
| Sharp | For multi-hop relay case, *sl-L2U2N-MH-Relay* should be included in SIB12, before UE using the resource pool(s) for discovery transmission. | Add the description in 5.2.2.4.13 Actions upon reception of *SIB12* 5.2.2.4.13 Actions upon reception of *SIB12* 3> if configured to transmit NR sidelink discovery:  4> if the UE is configured by upper layers to transmit NR sidelink L2 U2N relay discovery messages and *sl-L2U2N-Relay* is included in SIB12; or  4> for multi hop, if the UE is configured by upper layers to transmit NR sidelink L2 U2N relay discovery messages and *sl-L2U2N-MH-Relay* is included in SIB12; or  *<Omitted>*  5> use the resource pool(s) indicated by sl-DiscTxPoolSelected, sl-TxPoolExceptional or sl-TxPoolSelectedNormal for NR sidelink discovery transmission, as specified in 5.8.13.3; |
| Sharp | Section 5.8.9.8.3 is applied to L2 U2N relay UE  However the condition in yellow is applicable only for last relay UE.  Considering intermediate relay UE in connected state will enter this else part, the condition in yellow should be removed to avoid confusion.  2> else (the UE is in RRC\_CONNECTED on an active BWP without *pagingSearchSpace* configured): | 2> else ~~(the UE is in RRC\_CONNECTED on an active BWP without~~ *~~pagingSearchSpace~~* ~~configured)~~:  3> if the *sl-PagingInfo-RemoteUE* is set to *setup*:  4> include the received *sl-PagingIdentityRemoteUE* in *SidelinkUEInformationNR* message and perform Sidelink UE information transmission in accordance with 5.8.3;  3> else (the *sl-PagingInfo-RemoteUE* is set to *release*):  4> initiate transmission of the *SidelinkUEInformationNR* message to release the *sl-PagingIdentityRemoteUE* in *SidelinkUEInformationNR* message in accordance with 5.8.3;  4> release the received paging information in *sl-PagingInfo-RemoteUE*; |