**Source: Huawei (Rapporteur)**

**Title: KI#4 and KI#5, key questions for company view collection**

This document is to collect company views on key questions of KI#4 and #5 to facilitate the following conclusion discussion. Please kindly provide your company views on the following questions before EoB of Sep 16th. The rapporteur will collect the views and propose summary/way forwards/SoH for further discussion afterwards.

### Q1: How does UPF identify DL PDU Set info?

* Option 1: use existing IETF RTP/SRTP RFC and draft
* Option 2: Define/extend N6 protocols to carry related info
  + Option 2.1: extend GTP-U protocol
  + Option 2.2: extend HTTP header (S2-2205830)
  + Option 2.3: extend RTP header
* Option 3: UPF implementation based on e.g. traffic characteristics.
* Option 4: UPF interacts with NWDAF(S2-2205838)

**[Company view]**

**Position:**

**Justification**:

### Q2. How to deliver PDU Set importance information to RAN:

* Option 1: use different QoS Flows with different priority level. PDU Set importance is mapped to existing QoS flow priority.
* Option 2: use one QoS flow for different PDU Set with different priority level
  + Option 2.1: use different sub-QoS Flow within one QoS Flow, and using sub-QoS flow Identifier in GTP-U header
  + Option 2.2: use PDU Set importance information in GTP-U header

**[Company view]**

**Position:**

**Justification**:

### Q3: Support to PDU Set dependency-based scheduling

* Option 1: Identify accurate dependency relationship between PDU Sets for scheduling.
* Option 2: In some scenario (e.g. closed GOP), the decoding of the non-I frames between two successive I frames always directly or indirectly relies on the 1st I frame of the two successive I frames. If the 1st I frame is in error, the non-I frames can be dropped until the next I frame. (proposed in S2-2205839)
* Option 3: If a PDU Set is depended by others, it can be considered as more important during scheduling. But the scheduling will not further consider the accurate dependency relationship.

**[Company view]**

**Position:**

**Justification**:

### Q4. Support to hierarchical PDU Set:

* Option 1: introduces PDU Set group. (S2-2205938)
* Option 2: not support.

**[Company view]**

**Position:**

**Justification**:

### Q5. On “*Whether to drop a PDU Set in case PSDB is exceeded*”, do we need further define “*PDU Set Discard Time*” (A PDU Set shall be dropped in case this time is exceeded (sol 25 etc):

* Option 1: Support
* Option 2: not support.

**[Company view]**

**Position:**

**Justification**: