**3GPP TSG-SA3 Meeting #111 *S3-23xxxx***

**Berlin, Germany, 22 -26 May 2023**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  |  | **CR** |  | **rev** |  | **Current version:** |  |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **x** |

|  |
| --- |
|  |
| ***Title:***  | Clarification of NSSAA revocation |
|  |  |
| ***Source to WG:*** | Federal Office for Information Security (BSI) |
| ***Source to TSG:*** | S3 |
|  |  |
| ***Work item code:*** |  |  | ***Date:*** | 2023-05-08 |
|  |  |  |  |  |
| ***Category:*** | F |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | The UE state (REGISTERED) required for the test case is not present in the Pre-Conditions.The Requirement Description mentions, that the Deregistration Request message shall include the list of rejected S-NSSAIs, each of them with the appropriate rejection cause value. This is currently missing and should be part of the Expected Results. |
|  |  |
| ***Summary of change:*** | Added UE state to Pre-conditions.Added required content of Deregistration Request to Expected Results. |
|  |  |
| ***Consequences if not approved:*** | The state of the UE may not be correct while testing.Requirement Description is not covered fully. |
|  |  |
| ***Clauses affected:*** | 4.2.2.9.1 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **x** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **x** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **x** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

\*\*\*\*\*\*\*\*\*\* START OF 1st CHANGE \*\*\*\*\*\*\*\*\*\*

##### 4.2.2.9.1 NSSAA revocation

*Requirement Name*: NSSAA revocation

*Requirement Reference:* TS 33.501 [7], clause 16.5

*Requirement Description*: " If no S-NSSAI is left in Allowed NSSAI for an access after the revocation, and no Default NSSAI can be provided to the UE in the Allowed NSSAI or a previous NSSAA failed for the Default NSSAI over this access, then the AMF shall execute the Network-initiated Deregistration procedure for the access as described in subclause 4.2.2.3.3 in TS 23.502 [8], and it shall include in the explicit De-Registration Request message the list of Rejected S-NSSAIs, each of them with the appropriate rejection cause value. "

as specified in TS 33.501[7], clause 16.5

*Threat References*: TR 33.926, clause K.2.X

*Test Case*:

**Test Name:** TC\_NSSAA\_REVOCATION

**Purpose:**

Verify that AMF deregisters UE when, after slice specific authorization revocation, there is no allowed NSSAI or Default NSSAI that can be used by UE.

**Pre-Conditions:**

 - Test environment with UE. The UE may be simulated.

 - The UE is registered at the AMF.

 - The AMF under test is configured with one S-NSSAI in the Allowed NSSAI and no default S-NSSAI.

**Execution Steps**

A message requesting the AMF under test to revoke the authorization of the S-NSSAI in the Allowed NSSAI is simulated and sent the AMF under test.

**Expected Results:**

The Deregistration Request message is sent by the AMF under test to the UE.

The Deregistration Request message includes the list of rejected S-NSSAIs, each of them with the appropriate rejection cause value.

**Expected format of evidence:**

Evidence suitable for the interface, e.g., Screenshot containing the operational results.

NOTE 1: This test case is only applicable to AMF supporting Network Slice Specific Authentication and Authorization.

\*\*\*\*\*\*\*\*\*\* END OF CHANGE \*\*\*\*\*\*\*\*\*\*