{"text_format":"1","workbook":"xlsx","n_sheets":4,"sheets":["Cover","Parameters","PUSCH requirement 4Rx","PUSCH requirement 8Rx"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Cover","index":0,"n_rows":7,"n_cols":10,"rows_kept":7,"cut":false,"hidden":false,"merged":[]}
[]
[null,"3GPP TSG-RAN WG4 Meeting #117",null,null,null,null,null,null,null,"R4-2521037 "]
[null,"Dallas, Texas, USA, 17th Nov- 21st Nov, 2025"]
[]
[null,"Source: Ericsson"]
[null,"Title: Simulation results summary for 3Tx BS Demodulation requirements"]
[null,"Agenda: 6.12.3"]

{"sheet":"Parameters","index":1,"n_rows":12,"n_cols":5,"rows_kept":12,"cut":false,"hidden":false,"merged":[[1,2,1,4],[6,2,6,4],[7,2,7,4]]}
[]
[null,null,"Parameters for deriving performance requirements"]
[null,null,"Ideal Span Threshold",2,"dB"]
[null,null,"Impairment Span Threshold",4,"dB"]
[]
[]
[null,"Notes","1. Call function DerivingPerfReq()"]
[null,null,"2. If the ruls does not apply, or fails, -100dB or less will be returned"]
[null,null,null,-100,"Not enough input"]
[null,null,null,-101,"Input should be pairs"]
[null,null,null,-102,"Too large span for impairment"]
[null,null,null,-103,"After removal iteration, not enough input"]

{"sheet":"PUSCH requirement 4Rx","index":2,"n_rows":41,"n_cols":21,"rows_kept":41,"cut":false,"hidden":false,"merged":[[32,8,33,8],[35,1,36,1],[35,2,36,2],[35,3,36,3],[35,4,36,4],[35,6,36,6],[35,7,36,7],[35,8,36,8],[18,6,19,6],[18,7,19,7],[18,8,19,8],[39,1,40,1],[39,2,40,2],[39,3,40,3],[39,4,40,4],[39,6,40,6],[39,7,40,7],[39,8,40,8],[32,1,33,1],[32,2,33,2],[32,3,33,3],[32,4,33,4],[32,6,33,6],[32,7,33,7],[29,8,30,8],[26,8,27,8],[23,8,24,8],[5,8,6,8],[2,8,3,8],[8,8,9,8],[11,8,12,8],[14,8,15,8],[0,17,0,18],[0,19,0,20],[21,11,21,12],[21,13,21,14],[21,15,21,16],[21,17,21,18],[21,19,21,20],[0,11,0,12],[0,13,0,14],[0,15,0,16],[2,2,3,2],[5,2,6,2],[23,2,24,2],[26,2,27,2],[29,2,30,2],[8,2,9,2],[11,2,12,2],[14,2,15,2],[18,2,19,2],[2,1,3,1],[5,1,6,1],[23,1,24,1],[26,1,27,1],[29,1,30,1],[8,1,9,1],[11,1,12,1],[14,1,15,1],[18,1,19,1],[2,4,3,4],[5,4,6,4],[23,4,24,4],[26,4,27,4],[29,4,30,4],[8,4,9,4],[11,4,12,4],[14,4,15,4],[18,4,19,4],[2,3,3,3],[5,3,6,3],[23,3,24,3],[26,3,27,3],[29,3,30,3],[8,3,9,3],[11,3,12,3],[14,3,15,3],[18,3,19,3],[29,6,30,6],[8,6,9,6],[2,7,3,7],[5,7,6,7],[23,7,24,7],[26,7,27,7],[29,7,30,7],[8,7,9,7],[11,6,12,6],[11,7,12,7],[2,6,3,6],[5,6,6,6],[23,6,24,6],[26,6,27,6],[14,6,15,6],[14,7,15,7]]}
["case ","Tx","SCS","Waveform","BW","Mapping Type","Propagation condition ","MCS","Additional DM-RS position","38.104 req","38.141-1/2 req","Samsung",null,"Nokia",null,"Ericsson",null,"SPAN",null,"AVERAGE"]
[null,null,null,null,null,null,null,null,null,null,null,"ideal","Impairment","ideal","Impairment","ideal","Impairment","Ideal","Impairment","Ideal","Impairment"]
[1,3,"15kHz","CP-OFDM","5MHz","A","TDLB100-400",2,"pos1",{"$f":"DerivingPerfReq(L3:Q3)","v":-100},{"$f":"IF(J3>-100,J3+0.9,J3)","v":-100},-1.4319999999999999,null,-3.69,null,-2.71,null,{"$f":"MAX(L3,N3,P3)-MIN(L3,N3,P3)","v":2.258},{"$f":"MAX(M24,O24,Q24)","v":0},{"$f":"AVERAGE(L3,N3,P3)","v":-2.6106666666666665},{"$f":"AVERAGE(M3,O3,Q3)","v":{"$error":"#DIV/0!"}}]
[2,null,null,null,null,"B",null,null,null,{"$f":"DerivingPerfReq(L4:Q4)","v":-100},{"$f":"IF(J4>-100,J4+0.9,J4)","v":-100},null,null,-3.61,null,-2.59,null,{"$f":"MAX(L4,N4,P4)-MIN(L4,N4,P4)","v":1.02},{"$f":"MAX(M25,O25,Q25)","v":0},{"$f":"AVERAGE(L4,N4,P4)","v":-3.0999999999999996},{"$f":"AVERAGE(M4,O4,Q4)","v":{"$error":"#DIV/0!"}}]
[]
[3,3,"15kHz","CP-OFDM","5MHz","A","TDLC300-100",16,"pos1",{"$f":"DerivingPerfReq(L6:Q6)","v":-100},{"$f":"IF(J6>-100,J6+0.9,J6)","v":-100},13.593999999999999,null,8.4499999999999993,null,12.78,null,5.1440000000000001,{"$f":"MAX(M27,O27,Q27)","v":0},11.607999999999999,{"$error":"#DIV/0!"}]
[4,null,null,null,null,"B",null,null,null,{"$f":"DerivingPerfReq(L7:Q7)","v":-100},{"$f":"IF(J7>-100,J7+0.9,J7)","v":-100},null,null,8.6999999999999993,null,12.86,null,4.16,{"$f":"MAX(M28,O28,Q28)","v":0},10.78,{"$error":"#DIV/0!"}]
[]
[5,3,"15kHz","CP-OFDM","5MHz","A","TDLA30-10",20,"pos1",{"$f":"DerivingPerfReq(L9:Q9)","v":-100},{"$f":"IF(J9>-100,J9+0.9,J9)","v":-100},15.016,null,12.07,null,14.29,null,2.9459999999999997,{"$f":"MAX(M30,O30,Q30)","v":0},13.792,{"$error":"#DIV/0!"}]
[6,null,null,null,null,"B",null,null,null,{"$f":"DerivingPerfReq(L10:Q10)","v":-100},{"$f":"IF(J10>-100,J10+0.9,J10)","v":-100},null,null,12.12,null,14.28,null,2.16,{"$f":"MAX(M31,O31,Q31)","v":0},13.2,{"$error":"#DIV/0!"}]
[]
[7,3,"15kHz","CP-OFDM","50MHz","A","TDLB100-400",2,"pos1",{"$f":"DerivingPerfReq(L12:Q12)","v":-100},{"$f":"IF(J12>-100,J12+0.9,J12)","v":-100},-1.5209999999999999,null,-3.65,null,-2.73,null,2.129,{"$f":"MAX(M33,O33,Q33)","v":0},-2.6336666666666666,{"$error":"#DIV/0!"}]
[8,null,null,null,null,"B",null,null,null,{"$f":"DerivingPerfReq(L13:Q13)","v":-100},{"$f":"IF(J13>-100,J13+0.9,J13)","v":-100},null,null,-3.55,null,-2.54,null,1.0099999999999998,{"$f":"MAX(M34,O34,Q34)","v":0},-3.0449999999999999,{"$error":"#DIV/0!"}]
[]
[9,3,"15kHz","CP-OFDM","50MHz","A","TDLC300-100",16,"pos1",{"$f":"DerivingPerfReq(L15:Q15)","v":-100},{"$f":"IF(J15>-100,J15+0.9,J15)","v":-100},14.7,null,8.89,null,13.19,null,5.8099999999999987,{"$f":"MAX(M36,O36,Q36)","v":0},12.26,{"$error":"#DIV/0!"}]
[10,null,null,null,null,"B",null,null,null,{"$f":"DerivingPerfReq(L16:Q16)","v":-100},{"$f":"IF(J16>-100,J16+0.9,J16)","v":-100},null,null,8.91,null,13.31,null,4.4000000000000004,{"$f":"MAX(M37,O37,Q37)","v":0},11.11,{"$error":"#DIV/0!"}]
[]
[32,null,null,null,null,"B",null,null,null,{"$f":"DerivingPerfReq(L18:Q18)","v":-100},null,null,null,null,null,null,null,0,{"$f":"MAX(M39,O39,Q39)","v":0},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[11,3,"15kHz","CP-OFDM","50MHz","A","TDLA30-10",20,"pos1",{"$f":"DerivingPerfReq(L19:Q19)","v":-100},{"$f":"IF(J19>-100,J19+0.9,J19)","v":-100},17.251999999999999,null,12.91,null,16.149999999999999,null,4.3419999999999987,{"$f":"MAX(M40,O40,Q40)","v":0},15.437333333333333,{"$error":"#DIV/0!"}]
[12,null,null,null,null,"B",null,null,null,{"$f":"DerivingPerfReq(L20:Q20)","v":-100},{"$f":"IF(J20>-100,J20+0.9,J20)","v":-100},null,null,12.85,null,16.14,null,3.2900000000000009,{"$f":"MAX(M41,O41,Q41)","v":0},14.495000000000001,{"$error":"#DIV/0!"}]
[]
["case ","Tx","SCS","Waveform","BW","Mapping Type","Propagation condition ","MCS","Additional DM-RS position","38.104 req","38.141-1/2 req","Samsung",null,"Nokia",null,"Ericsson",null,"SPAN",null,"AVERAGE"]
[null,null,null,null,null,null,null,null,null,null,null,"ideal","Impairment","ideal","Impairment","ideal","Impairment","Ideal","Impairment","Ideal","Impairment"]
[1,3,"30kHz","CP-OFDM","10MHz","A","TDLB100-400",2,"pos1",{"$f":"DerivingPerfReq(L24:Q24)","v":-100},{"$f":"IF(J24>-100,J24+0.9,J24)","v":-100},-1.669,null,null,null,-2.74,null,{"$f":"MAX(L24,N24,P24)-MIN(L24,N24,P24)","v":1.0710000000000002},{"$f":"MAX(M45,O45,Q45)","v":0},{"$f":"AVERAGE(L24,N24,P24)","v":-2.2045000000000003},{"$f":"AVERAGE(M24,O24,Q24)","v":{"$error":"#DIV/0!"}}]
[2,null,null,null,null,"B",null,null,null,{"$f":"DerivingPerfReq(L25:Q25)","v":-100},{"$f":"IF(J25>-100,J25+0.9,J25)","v":-100},null,null,null,null,-2.72,null,{"$f":"MAX(L25,N25,P25)-MIN(L25,N25,P25)","v":0},{"$f":"MAX(M46,O46,Q46)","v":0},{"$f":"AVERAGE(L25,N25,P25)","v":-2.72},{"$f":"AVERAGE(M25,O25,Q25)","v":{"$error":"#DIV/0!"}}]
[]
[3,3,"30kHz","CP-OFDM","10MHz","A","TDLC300-100",16,"pos1",{"$f":"DerivingPerfReq(L27:Q27)","v":-100},{"$f":"IF(J27>-100,J27+0.9,J27)","v":-100},13.712,null,null,null,13.29,null,0.4220000000000006,{"$f":"MAX(M48,O48,Q48)","v":0},13.500999999999999,{"$error":"#DIV/0!"}]
[4,null,null,null,null,"B",null,null,null,{"$f":"DerivingPerfReq(L28:Q28)","v":-100},{"$f":"IF(J28>-100,J28+0.9,J28)","v":-100},null,null,null,null,13.44,null,0,{"$f":"MAX(M49,O49,Q49)","v":0},13.44,{"$error":"#DIV/0!"}]
[]
[5,3,"30kHz","CP-OFDM","10MHz","A","TDLA30-10",20,"pos1",{"$f":"DerivingPerfReq(L30:Q30)","v":-100},{"$f":"IF(J30>-100,J30+0.9,J30)","v":-100},15.09,null,null,null,14.43,null,0.66000000000000014,{"$f":"MAX(M51,O51,Q51)","v":0},14.76,{"$error":"#DIV/0!"}]
[6,null,null,null,null,"B",null,null,null,{"$f":"DerivingPerfReq(L31:Q31)","v":-100},{"$f":"IF(J31>-100,J31+0.9,J31)","v":-100},null,null,null,null,14.43,null,0,{"$f":"MAX(M52,O52,Q52)","v":0},14.43,{"$error":"#DIV/0!"}]
[]
[7,3,"30kHz","CP-OFDM","100MHz","A","TDLB100-400",2,"pos1",{"$f":"DerivingPerfReq(L33:Q33)","v":-100},{"$f":"IF(J33>-100,J33+0.9,J33)","v":-100},-1.724,null,null,null,-3.02,null,1.296,{"$f":"MAX(M64,O64,Q64)","v":0},-2.3719999999999999,{"$error":"#DIV/0!"}]
[8,null,null,null,null,"B",null,null,null,{"$f":"DerivingPerfReq(L34:Q34)","v":-100},{"$f":"IF(J34>-100,J34+0.9,J34)","v":-100},null,null,null,null,-2.99,null,0,0,-2.99,{"$error":"#DIV/0!"}]
[]
[9,3,"30kHz","CP-OFDM","100MHz","A","TDLC300-100",16,"pos1",{"$f":"DerivingPerfReq(L36:Q36)","v":-100},{"$f":"IF(J36>-100,J36+0.9,J36)","v":-100},14.371,null,null,null,14.25,null,0.12100000000000044,0,14.310500000000001,{"$error":"#DIV/0!"}]
[10,null,null,null,null,"B",null,null,null,{"$f":"DerivingPerfReq(L37:Q37)","v":-100},{"$f":"IF(J37>-100,J37+0.9,J37)","v":-100},null,null,null,null,14.37,null,0,0,14.37,{"$error":"#DIV/0!"}]
[]
[32,null,null,null,null,"B",null,null,null,{"$f":"DerivingPerfReq(L39:Q39)","v":-100},null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[11,3,"30kHz","CP-OFDM","100MHz","A","TDLA30-10",20,"pos1",{"$f":"DerivingPerfReq(L40:Q40)","v":-100},{"$f":"IF(J40>-100,J40+0.9,J40)","v":-100},16.899999999999999,null,null,null,16.149999999999999,null,0.75,0,16.524999999999999,{"$error":"#DIV/0!"}]
[12,null,null,null,null,"B",null,null,null,{"$f":"DerivingPerfReq(L41:Q41)","v":-100},{"$f":"IF(J41>-100,J41+0.9,J41)","v":-100},null,null,null,null,16.149999999999999,null,0,0,16.149999999999999,{"$error":"#DIV/0!"}]

{"sheet":"PUSCH requirement 8Rx","index":3,"n_rows":41,"n_cols":21,"rows_kept":41,"cut":false,"hidden":false,"merged":[[32,8,33,8],[35,1,36,1],[35,2,36,2],[35,3,36,3],[35,4,36,4],[35,6,36,6],[35,7,36,7],[35,8,36,8],[32,1,33,1],[32,2,33,2],[32,3,33,3],[32,4,33,4],[32,6,33,6],[32,7,33,7],[39,8,40,8],[39,1,40,1],[39,2,40,2],[39,3,40,3],[39,4,40,4],[39,6,40,6],[39,7,40,7],[29,8,30,8],[29,1,30,1],[29,2,30,2],[29,3,30,3],[29,4,30,4],[29,6,30,6],[29,7,30,7],[23,8,24,8],[26,1,27,1],[26,2,27,2],[26,3,27,3],[26,4,27,4],[26,6,27,6],[26,7,27,7],[26,8,27,8],[23,1,24,1],[23,2,24,2],[23,3,24,3],[23,4,24,4],[23,6,24,6],[23,7,24,7],[21,19,21,20],[18,1,19,1],[18,2,19,2],[18,3,19,3],[18,4,19,4],[18,6,19,6],[18,7,19,7],[18,8,19,8],[21,11,21,12],[21,13,21,14],[21,15,21,16],[21,17,21,18],[11,8,12,8],[14,1,15,1],[14,2,15,2],[14,3,15,3],[14,4,15,4],[14,6,15,6],[14,7,15,7],[14,8,15,8],[11,1,12,1],[11,2,12,2],[11,3,12,3],[11,4,12,4],[11,6,12,6],[11,7,12,7],[8,8,9,8],[8,1,9,1],[8,2,9,2],[8,3,9,3],[8,4,9,4],[8,6,9,6],[8,7,9,7],[2,7,3,7],[2,8,3,8],[5,1,6,1],[5,2,6,2],[5,3,6,3],[5,4,6,4],[5,6,6,6],[5,7,6,7],[5,8,6,8],[2,1,3,1],[2,2,3,2],[2,3,3,3],[2,4,3,4],[2,6,3,6],[0,11,0,12],[0,13,0,14],[0,15,0,16],[0,17,0,18],[0,19,0,20]]}
["case ","Tx","SCS","Waveform","BW","Mapping Type","Propagation condition ","MCS","Additional DM-RS position","38.104 req","38.141-1/2 req","Samsung",null,"Nokia",null,"Ericsson",null,"SPAN",null,"AVERAGE"]
[null,null,null,null,null,null,null,null,null,null,null,"ideal","Impairment","ideal","Impairment","ideal","Impairment","Ideal","Impairment","Ideal","Impairment"]
[1,3,"15kHz","CP-OFDM","5MHz","A","TDLB100-400",2,"pos1",{"$f":"DerivingPerfReq(L3:Q3)","v":-100},{"$f":"IF(J3>-100,J3+0.9,J3)","v":-100},null,null,-6.33,null,-5.99,null,{"$f":"MAX(L3,N3,P3)-MIN(L3,N3,P3)","v":0.33999999999999986},{"$f":"MAX(M24,O24,Q24)","v":0},{"$f":"AVERAGE(L3,N3,P3)","v":-6.16},{"$f":"AVERAGE(M3,O3,Q3)","v":{"$error":"#DIV/0!"}}]
[2,null,null,null,null,"B",null,null,null,{"$f":"DerivingPerfReq(L4:Q4)","v":-100},{"$f":"IF(J4>-100,J4+0.9,J4)","v":-100},null,null,-6.16,null,-5.88,null,{"$f":"MAX(L4,N4,P4)-MIN(L4,N4,P4)","v":0.28000000000000025},{"$f":"MAX(M25,O25,Q25)","v":0},{"$f":"AVERAGE(L4,N4,P4)","v":-6.02},{"$error":"#DIV/0!"}]
[]
[3,3,"15kHz","CP-OFDM","5MHz","A","TDLC300-100",16,"pos1",{"$f":"DerivingPerfReq(L6:Q6)","v":-100},{"$f":"IF(J6>-100,J6+0.9,J6)","v":-100},null,null,4.09,null,7.13,null,3.04,{"$f":"MAX(M27,O27,Q27)","v":0},5.6099999999999994,{"$error":"#DIV/0!"}]
[4,null,null,null,null,"B",null,null,null,{"$f":"DerivingPerfReq(L7:Q7)","v":-100},{"$f":"IF(J7>-100,J7+0.9,J7)","v":-100},null,null,4.12,null,7.13,null,3.01,{"$f":"MAX(M28,O28,Q28)","v":0},5.625,{"$error":"#DIV/0!"}]
[]
[5,3,"15kHz","CP-OFDM","5MHz","A","TDLA30-10",20,"pos1",{"$f":"DerivingPerfReq(L9:Q9)","v":-100},{"$f":"IF(J9>-100,J9+0.9,J9)","v":-100},null,null,6.39,null,9.08,null,2.6900000000000004,{"$f":"MAX(M30,O30,Q30)","v":0},7.7349999999999994,{"$error":"#DIV/0!"}]
[6,null,null,null,null,"B",null,null,null,{"$f":"DerivingPerfReq(L10:Q10)","v":-100},{"$f":"IF(J10>-100,J10+0.9,J10)","v":-100},null,null,6.54,null,9.08,null,2.54,{"$f":"MAX(M31,O31,Q31)","v":0},7.8100000000000005,{"$error":"#DIV/0!"}]
[]
[13,3,"15kHz","CP-OFDM","50MHz","A","TDLB100-400",2,"pos1",{"$f":"DerivingPerfReq(L12:Q12)","v":-100},{"$f":"IF(J12>-100,J12+0.9,J12)","v":-100},null,null,-5.82,null,-6.29,null,0.46999999999999975,{"$f":"MAX(M33,O33,Q33)","v":0},-6.0549999999999997,{"$error":"#DIV/0!"}]
[14,null,null,null,null,"B",null,null,null,{"$f":"DerivingPerfReq(L13:Q13)","v":-100},{"$f":"IF(J13>-100,J13+0.9,J13)","v":-100},null,null,-5.77,null,-5.95,null,0.1800000000000006,{"$f":"MAX(M34,O34,Q34)","v":0},-5.8599999999999994,{"$error":"#DIV/0!"}]
[]
[15,3,"15kHz","CP-OFDM","50MHz","A","TDLC300-100",16,"pos1",{"$f":"DerivingPerfReq(L15:Q15)","v":-100},{"$f":"IF(J15>-100,J15+0.9,J15)","v":-100},null,null,4.3499999999999996,null,7.33,null,2.9800000000000004,{"$f":"MAX(M36,O36,Q36)","v":0},5.84,{"$error":"#DIV/0!"}]
[16,null,null,null,null,"B",null,null,null,{"$f":"DerivingPerfReq(L16:Q16)","v":-100},{"$f":"IF(J16>-100,J16+0.9,J16)","v":-100},null,null,4.3600000000000003,null,7.35,null,2.9899999999999993,{"$f":"MAX(M37,O37,Q37)","v":0},5.8550000000000004,{"$error":"#DIV/0!"}]
[]
[32,null,null,null,null,"B",null,null,null,{"$f":"DerivingPerfReq(L18:Q18)","v":-100},null,null,null,null,null,null,null,0,{"$f":"MAX(M39,O39,Q39)","v":0},{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[17,3,"15kHz","CP-OFDM","50MHz","A","TDLA30-10",20,"pos1",{"$f":"DerivingPerfReq(L19:Q19)","v":-100},{"$f":"IF(J19>-100,J19+0.9,J19)","v":-100},null,null,7.18,null,9.75,null,2.5700000000000003,{"$f":"MAX(M40,O40,Q40)","v":0},8.4649999999999999,{"$error":"#DIV/0!"}]
[18,null,null,null,null,"B",null,null,null,{"$f":"DerivingPerfReq(L20:Q20)","v":-100},{"$f":"IF(J20>-100,J20+0.9,J20)","v":-100},null,null,7.25,null,9.75,null,2.5,{"$f":"MAX(M41,O41,Q41)","v":0},8.5,{"$error":"#DIV/0!"}]
[]
["case ","Tx","SCS","Waveform","BW","Mapping Type","Propagation condition ","MCS","Additional DM-RS position","38.104 req","38.141-1/2 req","Samsung",null,"Nokia",null,"Ericsson",null,"SPAN",null,"AVERAGE"]
[null,null,null,null,null,null,null,null,null,null,null,"ideal","Impairment","ideal","Impairment","ideal","Impairment","Ideal","Impairment","Ideal","Impairment"]
[1,3,"30kHz","CP-OFDM","10MHz","A","TDLB100-400",2,"pos1",{"$f":"DerivingPerfReq(L24:Q24)","v":-100},{"$f":"IF(J24>-100,J24+0.9,J24)","v":-100},null,null,null,null,-5.88,null,{"$f":"MAX(L24,N24,P24)-MIN(L24,N24,P24)","v":0},{"$f":"MAX(M45,O45,Q45)","v":0},{"$f":"AVERAGE(L24,N24,P24)","v":-5.88},{"$f":"AVERAGE(M24,O24,Q24)","v":{"$error":"#DIV/0!"}}]
[2,null,null,null,null,"B",null,null,null,{"$f":"DerivingPerfReq(L25:Q25)","v":-100},{"$f":"IF(J25>-100,J25+0.9,J25)","v":-100},null,null,null,null,-5.85,null,{"$f":"MAX(L25,N25,P25)-MIN(L25,N25,P25)","v":0},{"$f":"MAX(M46,O46,Q46)","v":0},{"$f":"AVERAGE(L25,N25,P25)","v":-5.85},{"$error":"#DIV/0!"}]
[]
[3,3,"30kHz","CP-OFDM","10MHz","A","TDLC300-100",16,"pos1",{"$f":"DerivingPerfReq(L27:Q27)","v":-100},{"$f":"IF(J27>-100,J27+0.9,J27)","v":-100},null,null,null,null,7.25,null,0,{"$f":"MAX(M48,O48,Q48)","v":0},7.25,{"$error":"#DIV/0!"}]
[4,null,null,null,null,"B",null,null,null,{"$f":"DerivingPerfReq(L28:Q28)","v":-100},{"$f":"IF(J28>-100,J28+0.9,J28)","v":-100},null,null,null,null,7.28,null,0,{"$f":"MAX(M49,O49,Q49)","v":0},7.28,{"$error":"#DIV/0!"}]
[]
[5,3,"30kHz","CP-OFDM","10MHz","A","TDLA30-10",20,"pos1",{"$f":"DerivingPerfReq(L30:Q30)","v":-100},{"$f":"IF(J30>-100,J30+0.9,J30)","v":-100},null,null,null,null,9.24,null,0,{"$f":"MAX(M51,O51,Q51)","v":0},9.24,{"$error":"#DIV/0!"}]
[6,null,null,null,null,"B",null,null,null,{"$f":"DerivingPerfReq(L31:Q31)","v":-100},{"$f":"IF(J31>-100,J31+0.9,J31)","v":-100},null,null,null,null,9.24,null,0,{"$f":"MAX(M52,O52,Q52)","v":0},9.24,{"$error":"#DIV/0!"}]
[]
[13,3,"30kHz","CP-OFDM","100MHz","A","TDLB100-400",2,"pos1",{"$f":"DerivingPerfReq(L33:Q33)","v":-100},{"$f":"IF(J33>-100,J33+0.9,J33)","v":-100},null,null,null,null,-5.94,null,0,{"$f":"MAX(M64,O64,Q64)","v":0},-5.94,{"$error":"#DIV/0!"}]
[14,null,null,null,null,"B",null,null,null,{"$f":"DerivingPerfReq(L34:Q34)","v":-100},{"$f":"IF(J34>-100,J34+0.9,J34)","v":-100},null,null,null,null,-6.38,null,0,0,-6.38,{"$error":"#DIV/0!"}]
[]
[15,3,"30kHz","CP-OFDM","100MHz","A","TDLC300-100",16,"pos1",{"$f":"DerivingPerfReq(L36:Q36)","v":-100},{"$f":"IF(J36>-100,J36+0.9,J36)","v":-100},null,null,null,null,7.61,null,0,0,7.61,{"$error":"#DIV/0!"}]
[16,null,null,null,null,"B",null,null,null,{"$f":"DerivingPerfReq(L37:Q37)","v":-100},{"$f":"IF(J37>-100,J37+0.9,J37)","v":-100},null,null,null,null,7.67,null,0,0,7.67,{"$error":"#DIV/0!"}]
[]
[32,null,null,null,null,"B",null,null,null,{"$f":"DerivingPerfReq(L39:Q39)","v":-100},null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[17,3,"30kHz","CP-OFDM","100MHz","A","TDLA30-10",20,"pos1",{"$f":"DerivingPerfReq(L40:Q40)","v":-100},{"$f":"IF(J40>-100,J40+0.9,J40)","v":-100},null,null,null,null,9.94,null,0,0,9.94,{"$error":"#DIV/0!"}]
[18,null,null,null,null,"B",null,null,null,{"$f":"DerivingPerfReq(L41:Q41)","v":-100},{"$f":"IF(J41>-100,J41+0.9,J41)","v":-100},null,null,null,null,9.94,null,0,0,9.94,{"$error":"#DIV/0!"}]