{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Cover","Parameters","PUSCH requirement  UL muting"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Cover","index":0,"n_rows":7,"n_cols":10,"rows_kept":7,"cut":false,"hidden":false,"merged":[]}
[]
[null,"3GPP TSG-RAN WG4 Meeting #116",null,null,null,null,null,null,null,"R4-2515039"]
[null,"Prague, Czech, 13th-17th, Oct, 2025"]
[]
[null,"Source: Samsung"]
[null,"Title: Simulation results summary for SBFD demodulation"]
[null,"Agenda: 6.23"]

{"sheet":"Parameters","index":1,"n_rows":12,"n_cols":5,"rows_kept":12,"cut":false,"hidden":false,"merged":[[1,2,1,4],[6,2,6,4],[7,2,7,4]]}
[]
[null,null,"Parameters for deriving performance requirements"]
[null,null,"Ideal Span Threshold",2,"dB"]
[null,null,"Impairment Span Threshold",4,"dB"]
[]
[]
[null,"Notes","1. Call function DerivingPerfReq()"]
[null,null,"2. If the ruls does not apply, or fails, -100dB or less will be returned"]
[null,null,null,-100,"Not enough input"]
[null,null,null,-101,"Input should be pairs"]
[null,null,null,-102,"Too large span for impairment"]
[null,null,null,-103,"After removal iteration, not enough input"]

{"sheet":"PUSCH requirement  UL muting","index":2,"n_rows":54,"n_cols":34,"rows_kept":54,"cut":false,"hidden":false,"merged":[[0,15,0,17],[0,30,0,31],[0,32,0,33],[0,18,0,20],[0,21,0,23],[0,24,0,26],[0,27,0,29]]}
["case ","Tx","case","Tx","Rx","SCS","BW","Number of  muting symbol","mapping type","Propagation condition for target cell","Propagation conditon for interferer cell ","Number of Interferer cells","INR set","38.104 req","38.141-1/2 req","Samsung ",null,null,"ZTE",null,null,"Huawei",null,null,"Ericsson",null,null,"Nokia",null,null,"SPAN",null,"Average"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MMSE IRC without using muting ","MMSE IRC with using muting ","gain","MMSE IRC without using muting","MMSE IRC with using muting ","gain","MMSE IRC without using muting","MMSE IRC with using muting ","gain","MMSE IRC without using muting","MMSE IRC with using muting ","gain"," MMSE IRC without using muting","MMSE IRC with using muting","gain","Ideal","Impairment","Ideal","Impairment"]
[null,null,1,1,2,"30KHz","20MHz","2 (4,14) ","A","TDLC300-100","TDLC300-0",2,"(5,-5)",null,null,13.444000000000001,13.157999999999999,0.28599999999999998,12,11.5,{"$f":"S3-T3","v":0.5}]
[null,null,2,1,2,"30KHz","20MHz","2 (4,14)","A","TDLC300-100","TDLC300-0",2,"(9,-1)",null,null,14.653,14.375999999999999,0.27700000000000002,14.7,14.3,{"$f":"S4-T4","v":0.39999999999999858}]
[null,null,3,1,2,"30KHz","20MHz","2 (4,14)","A","TDLC300-100","TDLC300-0",2,"(-1,-1)",null,null,12.69,12.369,0.32100000000000001]
[null,null,4,1,2,"30KHz","20MHz","2 (4,14)","A","TDLC300-100","TDLC300-0",2,"(3,3)",null,null,13.59,13.297000000000001,0.29299999999999998]
[null,null,5,1,2,"30KHz","20MHz","1 (4)","A","TDLC300-100","TDLC300-0",2,"(5,-5)",null,null,12.907999999999999,12.682,0.22600000000000001,null,null,null,13.3,12.6,{"$f":"V7-W7","v":0.70000000000000107},12.27,12.2,{"$f":"Y7-Z7","v":7.0000000000000284E-2}]
[null,null,6,1,2,"30KHz","20MHz","1 (4)","A","TDLC300-100","TDLC300-0",2,"(9,-1)",null,null,14.212999999999999,14.058,0.155,null,null,null,14.5,13.7,0.80000000000000071,14.08,13.8,{"$f":"Y8-Z8","v":0.27999999999999936}]
[null,null,7,1,2,"30KHz","20MHz","1 (4)","A","TDLC300-100","TDLC300-0",2,"(-1,-1)",null,null,12.151999999999999,11.917999999999999,0.23400000000000001,null,null,null,12.6,12,0.59999999999999964,11.65,11.64,{"$f":"Y9-Z9","v":9.9999999999997868E-3}]
[null,null,8,1,2,"30KHz","20MHz","1 (4)","A","TDLC300-100","TDLC300-0",2,"(3,3)",null,null,13.055,12.849,0.20599999999999999,null,null,null,13.5,12.8,0.69999999999999929,13.17,13.03,{"$f":"Y10-Z10","v":0.14000000000000057}]
[null,null,9,1,2,"30KHz","20MHz","2 (2,12) ","B","TDLC300-100","TDLC300-0",2,"(5,-5)",null,null,13.429,13.144,0.28499999999999998]
[null,null,10,1,2,"30KHz","20MHz","2 (2,12)","B","TDLC300-100","TDLC300-0",2,"(9,-1)",null,null,14.589,14.3,0.28899999999999998]
[null,null,11,1,2,"30KHz","20MHz","2 (2,12)","B","TDLC300-100","TDLC300-0",2,"(-1,-1)",null,null,12.714,12.364000000000001,0.35]
[null,null,12,1,2,"30KHz","20MHz","2 (2,12)","B","TDLC300-100","TDLC300-0",2,"(3,3)",null,null,13.579000000000001,13.266999999999999,0.312]
[null,null,13,1,2,"30KHz","20MHz","1 (2)","B","TDLC300-100","TDLC300-0",2,"(5,-5)",null,null,12.909000000000001,12.685,0.224,null,null,null,13.3,12.6,0.70000000000000107]
[null,null,14,1,2,"30KHz","20MHz","1 (2)","B","TDLC300-100","TDLC300-0",2,"(9,-1)",null,null,14.157999999999999,13.971,0.187,null,null,null,14.5,13.7,0.80000000000000071]
[null,null,15,1,2,"30KHz","20MHz","1 (2)","B","TDLC300-100","TDLC300-0",2,"(-1,-1)",null,null,12.19,11.984,0.20599999999999999,null,null,null,12.6,12,0.59999999999999964]
[null,null,16,1,2,"30KHz","20MHz","1 (2)","B","TDLC300-100","TDLC300-0",2,"(3,3)",null,null,13.058999999999999,12.866,0.193,null,null,null,13.5,12.8,0.69999999999999929]
[]
[]
[null,null,1,1,4,"30KHz","20MHz","2 (4,14) ","A","TDLC300-100","TDLC300-0",2,"(5,-5)",null,null,8.2509999999999994,7.6070000000000002,0.64400000000000002,6.3,6,{"$f":"S21-T21","v":0.29999999999999982}]
[null,null,2,1,4,"30KHz","20MHz","2 (4,14)","A","TDLC300-100","TDLC300-0",2,"(9,-1)",null,null,8.4749999999999996,7.6820000000000004,0.79300000000000004,8,7.5,0.5]
[null,null,3,1,4,"30KHz","20MHz","2 (4,14)","A","TDLC300-100","TDLC300-0",2,"(-1,-1)",null,null,7.83,7.0650000000000004,0.76500000000000001]
[null,null,4,1,4,"30KHz","20MHz","2 (4,14)","A","TDLC300-100","TDLC300-0",2,"(3,3)",null,null,8.3689999999999998,7.6710000000000003,0.69799999999999995]
[null,null,5,1,4,"30KHz","20MHz","1 (4)","A","TDLC300-100","TDLC300-0",2,"(5,-5)",null,null,7.9489999999999998,7.4269999999999996,0.52200000000000002,null,null,null,null,null,null,7.31,7.27,{"$f":"Y25-Z25","v":4.0000000000000036E-2}]
[null,null,6,1,4,"30KHz","20MHz","1 (4)","A","TDLC300-100","TDLC300-0",2,"(9,-1)",null,null,8.0350000000000001,7.4219999999999997,0.61299999999999999,null,null,null,null,null,null,8.61,8.49,{"$f":"Y26-Z26","v":0.11999999999999922}]
[null,null,7,1,4,"30KHz","20MHz","1 (4)","A","TDLC300-100","TDLC300-0",2,"(-1,-1)",null,null,7.4790000000000001,6.9180000000000001,0.56100000000000005,null,null,null,null,null,null,6.93,6.98,{"$f":"Y27-Z27","v":-5.0000000000000711E-2}]
[null,null,8,1,4,"30KHz","20MHz","1 (4)","A","TDLC300-100","TDLC300-0",2,"(3,3)",null,null,8.0380000000000003,7.4820000000000002,0.55600000000000005,null,null,null,null,null,null,7.6,7.5,{"$f":"Y28-Z28","v":9.9999999999999645E-2}]
[null,null,9,1,4,"30KHz","20MHz","2 (2,12) ","B","TDLC300-100","TDLC300-0",2,"(5,-5)",null,null,8.2729999999999997,7.6390000000000002,0.63400000000000001]
[null,null,10,1,4,"30KHz","20MHz","2 (2,12)","B","TDLC300-100","TDLC300-0",2,"(9,-1)",null,null,8.5259999999999998,7.6950000000000003,0.83099999999999996]
[null,null,11,1,4,"30KHz","20MHz","2 (2,12)","B","TDLC300-100","TDLC300-0",2,"(-1,-1)",null,null,7.8470000000000004,7.06,0.78700000000000003]
[null,null,12,1,4,"30KHz","20MHz","2 (2,12)","B","TDLC300-100","TDLC300-0",2,"(3,3)",null,null,8.3870000000000005,7.7450000000000001,0.64200000000000002]
[null,null,13,1,4,"30KHz","20MHz","1 (2)","B","TDLC300-100","TDLC300-0",2,"(5,-5)",null,null,8.0289999999999999,7.5259999999999998,0.503]
[null,null,14,1,4,"30KHz","20MHz","1 (2)","B","TDLC300-100","TDLC300-0",2,"(9,-1)",null,null,8.0909999999999993,7.4649999999999999,0.626]
[null,null,15,1,4,"30KHz","20MHz","1 (2)","B","TDLC300-100","TDLC300-0",2,"(-1,-1)",null,null,7.5410000000000004,6.9720000000000004,0.56899999999999995]
[null,null,16,1,4,"30KHz","20MHz","1 (2)","B","TDLC300-100","TDLC300-0",2,"(3,3)",null,null,8.1509999999999998,7.6260000000000003,0.52500000000000002]
[]
[]
[null,null,1,1,8,"30KHz","20MHz","2 (4,13) ","A","TDLC300-100","TDLC300-0",2,"(5,-5)",null,null,6.9459999999999997,3.8679999999999999,3.0779999999999998]
[null,null,2,1,8,"30KHz","20MHz","2 (4,13)","A","TDLC300-100","TDLC300-0",2,"(9,-1)",null,null,6.8860000000000001,4.0469999999999997,2.839]
[null,null,3,1,8,"30KHz","20MHz","2 (4,13)","A","TDLC300-100","TDLC300-0",2,"(-1,-1)",null,null,7.0350000000000001,3.9079999999999999,3.1269999999999998]
[null,null,4,1,8,"30KHz","20MHz","2 (4,13)","A","TDLC300-100","TDLC300-0",2,"(3,3)",null,null,6.9850000000000003,3.8559999999999999,3.129]
[null,null,5,1,8,"30KHz","20MHz","1 (4)","A","TDLC300-100","TDLC300-0",2,"(5,-5)",null,null,6.5970000000000004,4.327,2.27,null,null,null,null,null,null,3.14,3.23,{"$f":"Y43-Z43","v":-8.9999999999999858E-2}]
[null,null,6,1,8,"30KHz","20MHz","1 (4)","A","TDLC300-100","TDLC300-0",2,"(9,-1)",null,null,6.4939999999999998,4.3970000000000002,2.097,null,null,null,null,null,null,5.14,5.39,{"$f":"Y44-Z44","v":-0.25}]
[null,null,7,1,8,"30KHz","20MHz","1 (4)","A","TDLC300-100","TDLC300-0",2,"(-1,-1)",null,null,6.6539999999999999,4.3540000000000001,2.2999999999999998,null,null,null,null,null,null,1.64,1.81,{"$f":"Y45-Z45","v":-0.17000000000000015}]
[null,null,8,1,8,"30KHz","20MHz","1 (4)","A","TDLC300-100","TDLC300-0",2,"(3,3)",null,null,6.6150000000000002,4.2949999999999999,2.3199999999999998,null,null,null,null,null,null,3.47,3.62,{"$f":"Y46-Z46","v":-0.14999999999999991}]
[null,null,9,1,8,"30KHz","20MHz","2 (2,12) ","B","TDLC300-100","TDLC300-0",2,"(5,-5)",null,null,7.0110000000000001,3.8740000000000001,3.137]
[null,null,10,1,8,"30KHz","20MHz","2 (2,12)","B","TDLC300-100","TDLC300-0",2,"(9,-1)",null,null,6.87,3.9950000000000001,2.875]
[null,null,11,1,8,"30KHz","20MHz","2 (2,12)","B","TDLC300-100","TDLC300-0",2,"(-1,-1)",null,null,7.1260000000000003,3.9870000000000001,3.1389999999999998]
[null,null,12,1,8,"30KHz","20MHz","2 (2,12)","B","TDLC300-100","TDLC300-0",2,"(3,3)",null,null,7.0339999999999998,3.8570000000000002,3.177]
[null,null,13,1,8,"30KHz","20MHz","1 (2)","B","TDLC300-100","TDLC300-0",2,"(5,-5)",null,null,6.718,4.399,2.319]
[null,null,14,1,8,"30KHz","20MHz","1 (2)","B","TDLC300-100","TDLC300-0",2,"(9,-1)",null,null,6.5359999999999996,4.3959999999999999,2.14]
[null,null,15,1,8,"30KHz","20MHz","1 (2)","B","TDLC300-100","TDLC300-0",2,"(-1,-1)",null,null,6.82,4.4770000000000003,2.343]
[null,null,16,1,8,"30KHz","20MHz","1 (2)","B","TDLC300-100","TDLC300-0",2,"(3,3)",null,null,6.7469999999999999,4.3760000000000003,2.371]