{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Cover","Parameters","PUSCH requirement  UL muting"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Cover","index":0,"n_rows":7,"n_cols":10,"rows_kept":7,"cut":false,"hidden":false,"merged":[]}
[]
[null,"3GPP TSG-RAN WG4 Meeting #116",null,null,null,null,null,null,null,"R4-2515039"]
[null,"Prague, Czech, 13th-17th, Oct, 2025"]
[]
[null,"Source: Samsung"]
[null,"Title: Simulation results summary for SBFD demodulation"]
[null,"Agenda: 6.23"]

{"sheet":"Parameters","index":1,"n_rows":12,"n_cols":5,"rows_kept":12,"cut":false,"hidden":false,"merged":[[1,2,1,4],[6,2,6,4],[7,2,7,4]]}
[]
[null,null,"Parameters for deriving performance requirements"]
[null,null,"Ideal Span Threshold",2,"dB"]
[null,null,"Impairment Span Threshold",4,"dB"]
[]
[]
[null,"Notes","1. Call function DerivingPerfReq()"]
[null,null,"2. If the ruls does not apply, or fails, -100dB or less will be returned"]
[null,null,null,-100,"Not enough input"]
[null,null,null,-101,"Input should be pairs"]
[null,null,null,-102,"Too large span for impairment"]
[null,null,null,-103,"After removal iteration, not enough input"]

{"sheet":"PUSCH requirement  UL muting","index":2,"n_rows":36,"n_cols":34,"rows_kept":36,"cut":false,"hidden":false,"merged":[[0,15,0,17],[0,30,0,31],[0,32,0,33],[0,18,0,20],[0,21,0,23],[0,24,0,26],[0,27,0,29]]}
["case ","Tx","case","Tx","Rx","SCS","BW","Number of  muting symbol","mapping type","Propagation condition for target cell","Propagation conditon for interferer cell ","Number of Interferer cells","INR set","38.104 req","38.141-1/2 req","Samsung ",null,null,"ZTE",null,null,"Huawei",null,null,"Ericsson",null,null,"Nokia",null,null,"SPAN",null,"Average"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MMSE IRC without using muting ","MMSE IRC with using muting ","gain","MMSE IRC without using muting","MMSE IRC with using muting ","gain","MMSE IRC without using muting","MMSE IRC with using muting ","gain","MMSE IRC without using muting","MMSE IRC with using muting ","gain"," MMSE IRC without using muting","MMSE IRC with using muting","gain","Ideal","Impairment","Ideal","Impairment"]
[null,null,1,1,2,"30KHz","20MHz","2 (4,13) ","A","TDLC300-100","TDLC300-0",2,"(5,-5)",null,null,13.444000000000001,13.157999999999999,{"$f":"P3-Q3","v":0.28600000000000136},12.9,12.6,0.3]
[null,null,2,1,2,"30KHz","20MHz","2 (4,13)","A","TDLC300-100","TDLC300-0",2,"(9,-1)",null,null,14.653,14.375999999999999,{"$f":"P4-Q4","v":0.27700000000000102}]
[null,null,3,1,2,"30KHz","20MHz","2 (4,13)","A","TDLC300-100","TDLC300-0",2,"(13,3)",null,null,17.265999999999998,16.853999999999999,0.41199999999999903]
[null,null,4,1,2,"30KHz","20MHz","2 (4,13)","A","TDLC300-100","TDLC300-0",2,"(17,7)",null,null,20.661999999999999,19.77,0.89199999999999946,21.1,20.3,0.8]
[null,null,5,1,2,"30KHz","20MHz","2 (4,13)","A","TDLC300-100","TDLC300-0",2,"(-1,-1)",null,null,12.69,12.369,0.32099999999999973,11.7,11.3,0.4]
[null,null,6,1,2,"30KHz","20MHz","2 (4,13)","A","TDLC300-100","TDLC300-0",2,"(3,3)",null,null,13.59,13.297000000000001,0.29299999999999926]
[null,null,7,1,2,"30KHz","20MHz","2 (4,13)","A","TDLC300-100","TDLC300-0",2,"(7,7)",null,null,15.042999999999999,14.74,0.30299999999999905]
[null,null,8,1,2,"30KHz","20MHz","2 (4,13)","A","TDLC300-100","TDLC300-0",2,"(11,11)",null,null,17.835000000000001,17.309999999999999,0.52500000000000213,13.5,13.1,0.4]
[null,null,9,1,2,"30KHz","20MHz","1 (4)","A","TDLC300-100","TDLC300-0",2,"(5,-5)",null,null,12.907999999999999,12.682,0.22599999999999909]
[null,null,10,1,2,"30KHz","20MHz","1 (4)","A","TDLC300-100","TDLC300-0",2,"(9,-1)",null,null,14.212999999999999,14.058,0.15499999999999936]
[null,null,11,1,2,"30KHz","20MHz","1 (4)","A","TDLC300-100","TDLC300-0",2,"(13,3)",null,null,16.946999999999999,16.585999999999999,0.36100000000000065]
[null,null,12,1,2,"30KHz","20MHz","1 (4)","A","TDLC300-100","TDLC300-0",2,"(17,7)",null,null,20.209,19.411999999999999,0.7970000000000006]
[null,null,13,1,2,"30KHz","20MHz","1 (4)","A","TDLC300-100","TDLC300-0",2,"(-1,-1)",null,null,12.151999999999999,11.917999999999999,0.23399999999999999]
[null,null,14,1,2,"30KHz","20MHz","1 (4)","A","TDLC300-100","TDLC300-0",2,"(3,3)",null,null,13.055,12.849,0.20599999999999952]
[null,null,15,1,2,"30KHz","20MHz","1 (4)","A","TDLC300-100","TDLC300-0",2,"(7,7)",null,null,14.615,14.419,0.19599999999999973]
[null,null,16,1,2,"30KHz","20MHz","1 (4)","A","TDLC300-100","TDLC300-0",2,"(11,11)",null,null,17.434999999999999,17.068999999999999,0.36599999999999966]
[]
[]
[null,null,1,1,4,"30KHz","20MHz","2 (3,12) ","A","TDLC300-100","TDLC300-0",2,"(5,-5)"]
[null,null,2,1,4,"30KHz","20MHz","2 (3,12) ","A","TDLC300-100","TDLC300-0",2,"(9,-1)"]
[null,null,3,1,4,"30KHz","20MHz","2 (3,12) ","A","TDLC300-100","TDLC300-0",2,"(13,3)"]
[null,null,4,1,4,"30KHz","20MHz","2 (3,12) ","A","TDLC300-100","TDLC300-0",2,"(17,7)"]
[null,null,5,1,4,"30KHz","20MHz","2 (3,12) ","A","TDLC300-100","TDLC300-0",2,"(-1,-1)"]
[null,null,6,1,4,"30KHz","20MHz","2 (3,12) ","A","TDLC300-100","TDLC300-0",2,"(3,3)"]
[null,null,7,1,4,"30KHz","20MHz","2 (3,12) ","A","TDLC300-100","TDLC300-0",2,"(7,7)"]
[null,null,8,1,4,"30KHz","20MHz","2 (3,12) ","A","TDLC300-100","TDLC300-0",2,"(11,11)"]
[null,null,9,1,4,"30KHz","20MHz","1 (3)","A","TDLC300-100","TDLC300-0",2,"(5,-5)"]
[null,null,10,1,4,"30KHz","20MHz","1 (3)","A","TDLC300-100","TDLC300-0",2,"(9,-1)"]
[null,null,11,1,4,"30KHz","20MHz","1 (3)","A","TDLC300-100","TDLC300-0",2,"(13,3)"]
[null,null,12,1,4,"30KHz","20MHz","1 (3)","A","TDLC300-100","TDLC300-0",2,"(17,7)"]
[null,null,13,1,4,"30KHz","20MHz","1 (3)","A","TDLC300-100","TDLC300-0",2,"(-1,-1)"]
[null,null,14,1,4,"30KHz","20MHz","1 (3)","A","TDLC300-100","TDLC300-0",2,"(3,3)"]
[null,null,15,1,4,"30KHz","20MHz","1 (3)","A","TDLC300-100","TDLC300-0",2,"(7,7)"]
[null,null,16,1,4,"30KHz","20MHz","1 (3)","A","TDLC300-100","TDLC300-0",2,"(11,11)"]