{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Cover","Parameters","PUCCH format 2 UCI BLER"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Cover","index":0,"n_rows":7,"n_cols":10,"rows_kept":7,"cut":false,"hidden":false,"merged":[]}
[]
[null,"3GPP TSG-RAN WG4 Meeting #116-bis",null,null,null,null,null,null,null,"R4-250xxxx"]
[null,"Prague, Czech Republic, 13th-17th, Oct, 2025"]
[]
[null,"Source: Ericsson"]
[null,"Title: Simulation results summary for SAN PUCCH format 2 UCI BLER performance requirement "]
[null,"Agenda: 6.6.2.2"]

{"sheet":"Parameters","index":1,"n_rows":12,"n_cols":5,"rows_kept":12,"cut":false,"hidden":false,"merged":[[1,2,1,4],[6,2,6,4],[7,2,7,4]]}
[]
[null,null,"Parameters for deriving performance requirements"]
[null,null,"Ideal Span Threshold",2,"dB"]
[null,null,"Impairment Span Threshold",4,"dB"]
[]
[]
[null,"Notes","1. Call function DerivingPerfReq()"]
[null,null,"2. If the ruls does not apply, or fails, -100dB or less will be returned"]
[null,null,null,-100,"Not enough input"]
[null,null,null,-101,"Input should be pairs"]
[null,null,null,-102,"Too large span for impairment"]
[null,null,null,-103,"After removal iteration, not enough input"]

{"sheet":"PUCCH format 2 UCI BLER","index":2,"n_rows":4,"n_cols":20,"rows_kept":4,"cut":false,"hidden":false,"merged":[[0,10,0,11],[0,12,0,13],[0,14,0,15],[0,16,0,17],[0,18,0,19],[2,7,3,7],[2,2,3,2],[2,6,3,6],[2,1,3,1],[2,4,3,4],[2,3,3,3]]}
["case ","Tx","SCS","BW","Number of Tx antenna","Number of Rx antenna","Modulation order","Propagation condition for target cell","38.104 req","38.141-1/2 req","Samsung (R4-2513403)",null,"Huawei (R4-2510867)",null,"Ericsson (R4-2514019)",null,"SPAN",null,"Average"]
[null,null,null,null,null,null,null,null,null,null,"ideal","Impairment ","ideal ","Impairment","ideal","Impairment","Ideal","Impairment","Ideal","Impairment"]
[1,1,"15KHz","3MHz",1,1,"QPSK","NTN-TDLA100-200 Low",{"$f":"DerivingPerfReq(K3:P3)","v":-100},{"$f":"IF(I3>100, I3+0.6,I3)","v":-100},7.39,9.39,6.99,null,8.42,10.42,{"$f":"MAX(K3,M3,O3)-MIN(K3,M3,O3)","v":1.4299999999999997},{"$f":"MAX(L3,N3,P3)-MIN(L3,N3,P3)","v":1.0299999999999994},{"$f":"AVERAGE(K3,M3,O3)","v":7.5999999999999988},{"$f":"AVERAGE(L3,N3,P3)","v":9.9050000000000011}]
[2,null,null,null,null,2,null,null,{"$f":"DerivingPerfReq(K4:P4)","v":-100},{"$f":"IF(I4>100, I4+0.6,I4)","v":-100},0.53,2.5299999999999998,-0.13,null,0.79,2.79,{"$f":"MAX(K4,M4,O4)-MIN(K4,M4,O4)","v":0.92},{"$f":"MAX(L4,N4,P4)-MIN(L4,N4,P4)","v":0.26000000000000023},{"$f":"AVERAGE(K4,M4,O4)","v":0.39666666666666667},{"$f":"AVERAGE(L4,N4,P4)","v":2.66}]