3GPP TS 38.133 V15.20.0 (2022-12)

Technical Specification

3rd Generation Partnership Project;

Technical Specification Group Radio Access Network;

NR;

Requirements for support of radio resource management

(Release 15)

** 

The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP..  
The present document has not been subject to any approval process by the 3GPPOrganizational Partners and shall not be implemented.  
This Specification is provided for future development work within 3GPPonly. The Organizational Partners accept no liability for any use of this Specification.  
Specifications and Reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organizational Partners' Publications Offices.

***3GPP***

Postal address

3GPP support office address

650 Route des Lucioles - Sophia Antipolis

Valbonne - FRANCE

Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16

Internet

http://www.3gpp.org

***Copyright Notification***

No part may be reproduced except as authorized by written permission.  
The copyright and the foregoing restriction extend to reproduction in all media.

© 2022, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

UMTS™ is a Trade Mark of ETSI registered for the benefit of its members

3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  
LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners

GSM® and the GSM logo are registered and owned by the GSM Association

Contents

Foreword 30

1 Scope 31

2 References 31

3 Definitions, symbols and abbreviations 32

3.1 Definitions 32

3.2 Symbols 33

3.3 Abbreviations 34

3.4 Test tolerances 36

3.5 Frequency bands grouping 36

3.5.1 Introduction 36

3.5.2 NR operating bands in FR1 36

3.5.3 NR operating bands in FR2 36

3.6 Applicability of requirements in this specification version 37

3.6.1 RRC connected state requirements in DRX 37

3.6.2 Number of serving carriers 38

3.6.2.1 Number of serving carriers for SA 38

3.6.2.2 Number of serving carriers for EN-DC 38

3.6.2.3 Number of serving carriers for NE-DC 38

3.6.2.4 Number of serving carriers for NR-DC 38

3.6.3 Applicability for intra-band FR2 38

3.6.4 Applicability for FR2 UE power classes 39

3.6.5 Applicability for SDL bands 39

3.6.6 Applicability of requirements for NGEN-DC operation 39

3.6.7 Applicability of QCL 39

4 SA: RRC\_IDLE state mobility 39

4.1 Cell Selection 39

4.2 Cell Re-selection 39

4.2.1 Introduction 39

4.2.2 Requirements 40

4.2.2.1 UE measurement capability 40

4.2.2.2 Measurement and evaluation of serving cell 40

4.2.2.3 Measurements of intra-frequency NR cells 40

4.2.2.4 Measurements of inter-frequency NR cells 41

4.2.2.5 Measurements of inter-RAT E-UTRAN cells 43

4.2.2.6 Maximum interruption in paging reception 44

4.2.2.7 General requirements 44

5 SA: RRC\_INACTIVE state mobility 45

5.1 Cell Re-selection 45

5.1.1 Introduction 45

5.1.2 Requirements 45

5.1.2.1 UE measurement capability 45

5.1.2.2 Measurement and evaluation of serving cell 45

5.1.2.3 Measurements of intra-frequency NR cells 45

5.1.2.4 Measurements of inter-frequency NR cells 45

5.1.2.5 Measurements of inter-RAT E-UTRAN cells 45

5.1.2.6 Maximum interruption in paging reception 45

5.1.2.7 General requirements 45

5.2 Void 46

6 RRC\_CONNECTED state mobility 46

6.1 Handover 46

6.1.1 NR Handover 46

6.1.1.1 Introduction 46

6.1.1.2 NR FR1 - NR FR1 Handover 46

6.1.1.2.1 Handover delay 46

6.1.1.2.2 Interruption time 46

6.1.1.3 NR FR2- NR FR1 Handover 47

6.1.1.3.1 Handover delay 47

6.1.1.3.2 Interruption time 47

6.1.1.4 NR FR2- NR FR2 Handover 48

6.1.1.4.1 Handover delay 48

6.1.1.4.2 Interruption time 48

6.1.1.5 NR FR1- NR FR2 Handover 49

6.1.1.5.1 Handover delay 49

6.1.1.5.2 Interruption time 49

6.1.2 NR Handover to other RATs 50

6.1.2.1 NR – E-UTRAN Handover 50

6.1.2.1.1 Introduction 50

6.1.2.1.2 Handover delay 50

6.1.2.1.3 Interruption time 50

6.2 RRC Connection Mobility Control 51

6.2.1 SA: RRC Re-establishment 51

6.2.1.1 Introduction 51

6.2.1.2 Requirements 51

6.2.1.2.1 UE Re-establishment delay requirement 51

6.2.2 Random access 52

6.2.2.1 Introduction 52

6.2.2.2 Requirements 52

6.2.2.2.1 Contention based random access 53

6.2.2.2.2 Non-Contention based random access 54

6.2.2.2.3 UE behaviour when configured with supplementary UL 55

6.2.3 SA: RRC Connection Release with Redirection 55

6.2.3.1 Introduction 55

6.2.3.2 Requirements 55

6.2.3.2.1 RRC connection release with redirection to NR 55

6.2.3.2.2 RRC connection release with redirection to E-UTRAN 56

7 Timing 56

7.1 UE transmit timing 56

7.1.1 Introduction 56

7.1.2 Requirements 56

7.1.2.1 Gradual timing adjustment 57

7.1.2.2 Void 58

7.2 UE timer accuracy 58

7.2.1 Introduction 58

7.2.2 Requirements 58

7.3 Timing advance 58

7.3.1 Introduction 58

7.3.2 Requirements 59

7.3.2.1 Timing Advance adjustment delay 59

7.3.2.2 Timing Advance adjustment accuracy 59

7.4 Cell phase synchronization accuracy 59

7.4.1 Definition 59

7.4.2 Minimum requirements 59

7.5 Maximum Transmission Timing Difference 59

7.5.1 Introduction 59

7.5.2 Minimum Requirements for inter-band EN-DC 59

7.5.2.1 Minimum Requirements for inter-band synchronous EN-DC 60

7.5.3 Minimum Requirements for intra-band EN-DC 60

7.5.4 Minimum Requirements for NR Carrier Aggregation 61

7.5.5 Minimum Requirements for inter-band NE-DC 61

7.5.5.1 Minimum Requirements for inter-band synchronous NE-DC 61

7.5.6 Minimum Requirements for inter-band NR DC 62

7.6 Maximum Receive Timing Difference 62

7.6.1 Introduction 62

7.6.2 Minimum Requirements for inter-band EN-DC 62

7.6.2.1 Minimum Requirements for inter-band synchronous EN-DC 63

7.6.3 Minimum Requirements for intra-band EN-DC 63

7.6.4 Minimum Requirements for NR Carrier Aggregation 64

7.6.5 Minimum Requirements for inter-band NE-DC 64

7.6.5.1 Minimum Requirements for inter-band synchronous NE-DC 65

7.6.6 Minimum Requirements for inter-band NR DC 65

7.7 *deriveSSB-IndexFromCell* tolerance 65

7.7.1 Minimum requirements 65

7.8 Void 66

8 Signalling characteristics 66

8.1 Radio Link Monitoring 66

8.1.1 Introduction 66

8.1.2 Requirements for SSB based radio link monitoring 67

8.1.2.1 Introduction 67

8.1.2.2 Minimum requirement 68

8.1.2.3 Measurement restrictions for SSB based RLM 69

8.1.3 Requirements for CSI-RS based radio link monitoring 70

8.1.3.1 Introduction 70

8.1.3.2 Minimum requirement 70

8.1.3.3 Measurement restrictions for CSI-RS based RLM 72

8.1.4 Minimum requirement at transitions 73

8.1.5 Minimum requirement for UE turning off the transmitter 73

8.1.6 Minimum requirement for L1 indication 73

8.1.7 Scheduling availability of UE during radio link monitoring 74

8.1.7.1 Scheduling availability of UE performing radio link monitoring with a same subcarrier spacing as PDSCH/PDCCH on FR1 74

8.1.7.2 Scheduling availability of UE performing radio link monitoring with a different subcarrier spacing than PDSCH/PDCCH on FR1 74

8.1.7.3 Scheduling availability of UE performing radio link monitoring on FR2 74

8.1.7.4 Scheduling availability of UE performing radio link monitoring on FR1 or FR2 in case of FR1-FR2 inter-band CA and NR-DC 75

8.2 Interruption 75

8.2.1 EN-DC Interruption 75

8.2.1.1 Introduction 75

8.2.1.2 Requirements 76

8.2.1.2.1 Interruptions at transitions between active and non-active during DRX 76

8.2.1.2.2 Interruptions at transitions from non-DRX to DRX 76

8.2.1.2.3 Interruptions at SCell addition/release 76

8.2.1.2.4 Interruptions at SCell activation/deactivation 77

8.2.1.2.5 Interruptions during measurements on SCC 78

8.2.1.2.6 Interruptions at UL carrier RRC reconfiguration 79

8.2.1.2.7 Interruptions due to Active BWP switching Requirement 79

8.2.2 SA: Interruptions with Standalone NR Carrier Aggregation 80

8.2.2.1 Introduction 80

8.2.2.2 Requirements 80

8.2.2.2.1 Interruptions at SCell addition/release 80

8.2.2.2.2 Interruptions at SCell activation/deactivation 81

8.2.2.2.3 Interruptions during measurements on deactivated SCC 82

8.2.2.2.4 Interruptions at UL carrier RRC reconfiguration 82

8.2.2.2.5 Interruptions due to Active BWP switching Requirement 83

8.2.2.2.6 Interruptions at inter-frequency SFTD measurement 84

8.2.3 NE-DC Interruptions 85

8.2.3.1 Introduction 85

8.2.3.2 Requirements 85

8.2.3.2.1 Interruptions at transitions between active and non-active during DRX 85

8.2.3.2.2 Interruptions at transitions from non-DRX to DRX 86

8.2.3.2.3 Interruptions at PSCell/SCell addition/release 86

8.2.3.2.4 Interruptions at SCell activation/deactivation 87

8.2.3.2.5 Interruptions during measurements on SCC 88

8.2.3.2.6 Interruptions at UL carrier RRC reconfiguration 89

8.2.3.2.7 Interruptions due to Active BWP switching Requirement 89

8.2.4 NR-DC: Interruptions 89

8.2.4.1 Introduction 89

8.2.4.2 Requirements 90

8.2.4.2.1 Interruptions at PSCell/SCell addition/release 90

8.2.4.2.2 Interruptions at SCell activation/deactivation 90

8.2.4.2.3 Interruptions during measurements on SCC 91

8.2.4.2.4 Interruptions at UL carrier RRC reconfiguration 91

8.2.4.2.5 Interruptions due to Active BWP switching Requirement 92

8.2.4.2.6 Interruptions at transitions between active and non-active during DRX 92

8.2.4.2.7 Interruptions at transitions from non-DRX to DRX 92

8.3 SCell Activation and Deactivation Delay 92

8.3.1 Introduction 92

8.3.2 SCell Activation Delay Requirement for Deactivated SCell 93

8.3.3 SCell Deactivation Delay Requirement for Activated SCell 96

8.4 UE UL carrier RRC reconfiguration delay 97

8.4.1 Introduction 97

8.4.2 UE UL carrier configuration delay requirement 97

8.4.3 UE UL carrier deconfiguration delay requirement 97

8.5 Link Recovery Procedures 97

8.5.1 Introduction 97

8.5.2 Requirements for SSB based beam failure detection 98

8.5.2.1 Introduction 98

8.5.2.2 Minimum requirement 98

8.5.2.3 Measurement restriction for SSB based beam failure detection 100

8.5.3 Requirements for CSI-RS based beam failure detection 100

8.5.3.1 Introduction 100

8.5.3.2 Minimum requirement 101

8.5.3.3 Measurement restrictions for CSI-RS beam failure detection 103

8.5.4 Minimum requirement for L1 indication 103

8.5.5 Requirements for SSB based candidate beam detection 104

8.5.5.1 Introduction 104

8.5.5.2 Minimum requirement 104

8.5.5.3 Measurement restriction for SSB based candidate beam detection 106

8.5.6 Requirements for CSI-RS based candidate beam detection 106

8.5.6.1 Introduction 106

8.5.6.2 Minimum requirement 106

8.5.6.3 Measurement restriction for CSI-RS based candidate beam detection 108

8.5.7 Scheduling availability of UE during beam failure detection 109

8.5.7.1 Scheduling availability of UE performing beam failure detection with a same subcarrier spacing as PDSCH/PDCCH on FR1 109

8.5.7.2 Scheduling availability of UE performing beam failure detection with a different subcarrier spacing than PDSCH/PDCCH on FR1 109

8.5.7.3 Scheduling availability of UE performing beam failure detection on FR2 109

8.5.7.4 Scheduling availability of UE performing beam failure detection on FR1 or FR2 in case of FR1-FR2 inter-band CA and NR DC 110

8.5.8 Scheduling availability of UE during candidate beam detection 110

8.5.8.1 Scheduling availability of UE performing L1-RSRP measurement with a same subcarrier spacing as PDSCH/PDCCH on FR1 110

8.5.8.2 Scheduling availability of UE performing L1-RSRP measurement with a different subcarrier spacing than PDSCH/PDCCH on FR1 110

8.5.8.3 Scheduling availability of UE performing L1-RSRP measurement on FR2 110

8.5.8.4 Scheduling availability of UE performing L1-RSRP measurement on FR1 or FR2 in case of FR1-FR2 inter-band CA and NR-DC 111

8.5.9 Minimum requirement at transitions for beam failure detection 111

8.6 Active BWP switch delay 111

8.6.1 Introduction 111

8.6.2 DCI and timer based BWP switch delay 111

8.6.3 RRC based BWP switch delay 112

8.7 Void 113

8.8 NE-DC: E-UTRAN PSCell Addition and Release Delay 113

8.8.1 Introduction 113

8.8.2 E-UTRAN PSCell Addition Delay Requirement 113

8.8.3 E-UTRAN PSCell Release Delay Requirement 114

8.9 NR-DC: PSCell Addition and Release Delay 114

8.9.1 Introduction 114

8.9.2 PSCell Addition Delay Requirement 114

8.9.3 PSCell Release Delay Requirement 115

8.10 Active TCI state switching delay 115

8.10.6 Active TCI state list update delay 117

8.11 PSCell Change 117

9 Measurement Procedure 118

9.1 General measurement requirement 118

9.1.1 Introduction 118

9.1.2 Measurement gap 118

9.1.2.1 EN-DC: Measurement Gap Sharing 125

9.1.2.1a SA: Measurement Gap Sharing 126

9.1.2.1b NE-DC: Measurement Gap Sharing 127

9.1.2.1c NR-DC: Measurement Gap Sharing 127

9.1.3 UE Measurement capability 128

9.1.3.1 EN-DC: Monitoring of multiple layers using gaps 128

9.1.3.1a SA: Monitoring of multiple layers using gaps 129

9.1.3.1b NE-DC: Monitoring of multiple layers using gaps 129

9.1.3.1c NR-DC: Monitoring of multiple layers using gaps 129

9.1.3.2 EN-DC: Maximum allowed layers for multiple monitoring 130

9.1.3.2a SA: Maximum allowed layers for multiple monitoring 130

9.1.3.2b NE-DC: Maximum allowed layers for multiple monitoring 131

9.1.3.2c NR-DC: Maximum allowed layers for multiple monitoring 131

9.1.4 Capabilities for Support of Event Triggering and Reporting Criteria 132

9.1.4.1 Introduction 132

9.1.4.2 Requirements 132

9.1.5 Carrier-specific scaling factor 133

9.1.5.1 Monitoring of multiple layers outside gaps 133

9.1.5.1.1 EN-DC mode: carrier-specific scaling factor for SSB-based measurements performed outside gaps 134

9.1.5.1.2 SA mode: carrier-specific scaling factor for SSB-based measurements performed outside gaps 135

9.1.5.1.3 NR-DC mode: carrier-specific scaling factor for SSB-based measurements performed outside gaps 136

9.1.5.1.4 NE-DC mode: carrier-specific scaling factor for SSB-based measurements performed outside gaps 136

9.1.5.2 Monitoring of multiple layers within gaps 136

9.1.5.2.1 EN-DC mode: carrier-specific scaling factor for SSB-based measurements performed within gaps 137

9.1.5.2.2 SA mode: carrier-specific scaling factor for SSB-based measurements performed within gaps 138

9.1.5.2.3 NE-DC: carrier-specific scaling factor for SSB-based measurements performed within gaps 139

9.1.5.2.4 NR-DC: carrier-specific scaling factor for SSB-based measurements performed within gaps 141

9.1.6 Minimum requirement at transitions 142

9.2 NR intra-frequency measurements 142

9.2.1 Introduction 142

9.2.2 Requirements applicability 143

9.2.3 Number of cells and number of SSB 143

9.2.3.1 Requirements for FR1 143

9.2.3.2 Requirements for FR2 143

9.2.4 Measurement Reporting Requirements 144

9.2.4.1 Periodic Reporting 144

9.2.4.2 Event-triggered Periodic Reporting 144

9.2.4.3 Event Triggered Reporting 144

9.2.5 Intrafrequency measurements without measurement gaps 144

9.2.5.1 Intrafrequency cell identification 144

9.2.5.2 Measurement period 147

9.2.5.3 Scheduling availability of UE during intra-frequency measurements 148

9.2.5.3.1 Scheduling availability of UE performing measurements in TDD bands on FR1 148

9.2.5.3.2 Scheduling availability of UE performing measurements with a different subcarrier spacing than PDSCH/PDCCH on FR1 148

9.2.5.3.3 Scheduling availability of UE performing measurements on FR2 149

9.2.5.3.4 Scheduling availability of UE performing measurements on FR1 or FR2 in case of FR1-FR2 inter-band CA 150

9.2.5.4 SFTD Measurements between PCell and PSCell 150

9.2.5.4.1 Introduction 150

9.2.5.4.2 SFTD Measurement delay 150

9.2.5.4.3 SFTD Measurement Reporting Delay 151

9.2.6 Intra-frequency measurements with measurement gaps 151

9.2.6.1 Void 151

9.2.6.2 Intra-frequency cell identification 151

9.2.6.3 Intra-frequency Measurement Period 152

9.3 NR inter-frequency measurements 153

9.3.1 Introduction 153

9.3.2 Requirements applicability 153

9.3.2.1 Void 154

9.3.2.2 Void 154

9.3.3 Number of cells and number of SSB 154

9.3.3.1 Requirements for FR1 154

9.3.3.2 Requirements for FR2 154

9.3.4 Inter-frequency cell identification 154

9.3.4.1 Void 155

9.3.4.2 Void 155

9.3.5 Inter-frequency measurements 155

9.3.5.1 Void 156

9.3.5.2 Void 156

9.3.5.3 Void 156

9.3.6 Inter-frequency measurements reporting requirements 156

9.3.6.1 Periodic Reporting 156

9.3.6.2 Event-triggered Periodic Reporting 156

9.3.6.3 Event-triggered Reporting 156

9.3.7 Void 157

9.3.8 Inter-frequency SFTD measurement requirements 157

9.3.8.1 Introduction 157

9.3.8.2 SFTD Measurement delay 157

9.3.8.3 SFTD Measurement reporting delay 158

9.4 Inter-RAT measurements 158

9.4.1 Introduction 158

9.4.2 NR − E-UTRAN FDD measurements 159

9.4.2.1 Introduction 159

9.4.2.2 Requirements when no DRX is used 160

9.4.2.3 Requirements when DRX is used 160

9.4.2.4 Measurement reporting requirements 161

9.4.2.4.1 Periodic Reporting 161

9.4.2.4.2 Event-Triggered Periodic Reporting 161

9.4.2.4.3 Event-Triggered Reporting 161

9.4.3 NR − E-UTRAN TDD measurements 162

9.4.3.1 Introduction 162

9.4.3.2 Requirements when no DRX is used 162

9.4.3.3 Requirements when DRX is used 163

9.4.3.4 Measurement reporting requirements 164

9.4.3.4.1 Periodic Reporting 164

9.4.3.4.2 Event-Triggered Periodic Reporting 164

9.4.3.4.3 Event-Triggered Reporting 164

9.4.4 Inter-RAT RSTD measurements 164

9.4.4.1 NR − E-UTRAN FDD RSTD measurements 164

9.4.4.1.1 Introduction 164

9.4.4.1.2 Requirements 165

9.4.4.2 NR − E-UTRAN TDD RSTD measurements 168

9.4.4.2.1 Introduction 168

9.4.4.2.2 Requirements 169

9.4.5 Inter-RAT E-CID measurements 172

9.4.5.1 NR−E-UTRAN FDD E-CID RSRP and RSRQ measurements 172

9.4.5.1.1 Introduction 172

9.4.5.1.2 Requirements 172

9.4.5.1.3 Measurement Reporting Delay 172

9.4.5.2 NR−E-UTRAN TDD E-CID RSRP and RSRQ measurements 172

9.4.5.2.1 Introduction 172

9.4.5.2.2 Requirements 172

9.4.5.2.3 Measurement Reporting Delay 173

9.5 L1-RSRP measurements for Reporting 173

9.5.1 Introduction 173

9.5.2 Requirements applicability 173

9.5.3 Measurement Reporting Requirements 173

9.5.3.1 Periodic Reporting 174

9.5.3.2 Semi-Persistent Reporting 174

9.5.3.3 Aperiodic Reporting 174

9.5.4 L1-RSRP measurement requirements 174

9.5.4.1 SSB based L1-RSRP Reporting 174

9.5.4.2 CSI-RS based L1-RSRP Reporting 176

9.5.5 Measurement restriction for CSI-RS and SSB for L1-RSRP measurement 178

9.5.5.1 Measurement restriction for SSB based L1-RSRP 179

9.5.5.2 Measurement restriction for CSI-RS based L1-RSRP 179

9.5.6 Scheduling availability of UE during L1-RSRP measurement 180

9.5.6.1 Scheduling availability of UE performing L1-RSRP measurement with a same subcarrier spacing as PDSCH/PDCCH on FR1 180

9.5.6.2 Scheduling availability of UE performing L1-RSRP measurement with a different subcarrier spacing than PDSCH/PDCCH on FR1 180

9.5.6.3 Scheduling availability of UE performing L1-RSRP measurement on FR2 180

9.5.6.4 Scheduling availability of UE performing L1-RSRP measurement on FR1 or FR2 in case of FR1-FR2 inter-band CA 181

9.6 NE-DC: Measurements 181

9.6.1 Introduction 181

9.6.2 SFTD Measurements 181

9.6.2.1 Introduction 181

9.6.2.2 SFTD Measurement requirements 181

10 Measurement Performance requirements 182

10.1 NR measurements 182

10.1.1 Introduction 182

10.1.2 Intra-frequency RSRP accuracy requirements for FR1 183

10.1.2.1 Intra-frequency SS-RSRP accuracy requirements 183

10.1.2.1.1 Absolute SS-RSRP Accuracy 183

10.1.2.1.2 Relative SS-RSRP Accuracy 183

10.1.2.2 Void 184

10.1.3 Intra-frequency RSRP accuracy requirements for FR2 184

10.1.3.1 Intra-frequency SS-RSRP accuracy requirements 184

10.1.3.1.1 Absolute SS-RSRP Accuracy 184

10.1.3.1.2 Relative SS-RSRP Accuracy 185

10.1.3.2 Void 186

10.1.4 Inter-frequency RSRP accuracy requirements for FR1 186

10.1.4.1 Inter-frequency SS-RSRP accuracy requirements 186

10.1.4.1.1 Absolute Accuracy of SS-RSRP in FR1 186

10.1.4.1.2 Relative Accuracy of SS-RSRP in FR1 186

10.1.4.2 Void 187

10.1.5 Inter-frequency RSRP accuracy requirements for FR2 187

10.1.5.1 Inter-frequency SS-RSRP accuracy requirements 187

10.1.5.1.1 Absolute SS-RSRP Accuracy 187

10.1.5.1.2 Relative SS-RSRP Accuracy 188

10.1.5.2 Void 189

10.1.6 RSRP Measurement Report Mapping 189

10.1.7 Intra-frequency RSRQ accuracy requirements for FR1 191

10.1.7.1 Intra-frequency SS-RSRQ accuracy requirements in FR1 191

10.1.7.1.1 Absolute SS-RSRQ Accuracy in FR1 191

10.1.8 Intra-frequency RSRQ accuracy requirements for FR2 192

10.1.8.1 Intra-frequency SS-RSRQ accuracy requirements in FR2 192

10.1.8.1.1 Absolute SS-RSRQ Accuracy in FR2 192

10.1.9 Inter-frequency RSRQ accuracy requirements for FR1 193

10.1.9.1 Inter-frequency SS-RSRQ accuracy requirements in FR1 193

10.1.9.1.1 Aboslute Accuracy of SS-RSRQ in FR1 193

10.1.9.1.2 Relative Accuracy of SS-RSRQ in FR1 194

10.1.10 Inter-frequency RSRQ accuracy requirements for FR2 194

10.1.11 RSRQ report mapping 196

10.1.12 Intra-frequency SINR accuracy requirements for FR1 196

10.1.13 Intra-frequency SINR accuracy requirements for FR2 197

10.1.14 Inter-frequency SINR accuracy requirements for FR1 198

10.1.15 Inter-frequency SINR accuracy requirements for FR2 199

10.1.16 SINR report mapping 201

10.1.17 Power Headroom 201

10.1.18 PCMAX,c,f 202

10.1.19 L1-RSRP accuracy requirements for FR1 202

10.1.20 L1-RSRP accuracy requirements for FR2 206

10.1.21 SFTD accuracy requirements 209

10.2 E-UTRAN measurements 213

10.2.1 Introduction 213

10.2.2 E-UTRAN RSRP measurements 213

10.2.3 E-UTRAN RSRQ measurements 214

10.2.4 E-UTRAN RSTD measurements 214

10.2.5 E-UTRAN RS-SINR measurements 214

11 Void 214

Annex A (normative): Test Cases 212

A.1 Purpose of annex 212

A.2 Requirement classification for statistical testing 212

A.2.1 Types of requirements in TS 38.133 212

A.2.1.1 Time and delay requirements on UE higher layer actions 212

A.2.1.2 Measurements of power levels, relative powers and time 213

A.2.1.3 Implementation requirements 213

A.2.1.4 Physical layer timing requirements 213

A.3 RRM test configurations 214

A.3.1 Reference measurement channels 214

A.3.1.1 PDSCH 214

A.3.1.1.1 FDD 214

A.3.1.1.2 TDD 215

A.3.1.2 CORESET for RMSI scheduling 218

A.3.1.2.1 FDD 218

A.3.1.2.2 TDD 219

A.3.1.3 CORESET for RMC scheduling 222

A.3.1.3.1 FDD 222

A.3.1.3.2 TDD 223

A.3.1.4 TDD UL/DL configuration 226

A.3.2 OFDMA channel noise generator (OCNG) 227

A.3.2.1 Generic OFDMA Channel Noise Generator (OCNG) 227

A.3.2.1.1 OCNG pattern 1: Generic OCNG pattern for all unused REs 227

A.3.2.1.2 OCNG pattern 2: Generic OCNG pattern for all unused REs for 2AoA setup 228

A.3.2.1.3 OCNG pattern 3: Generic OCNG pattern for unused REs in the same bandwidth as CORESET 228

A.3.2.1.4 OCNG pattern 4: Generic OCNG pattern for all unused REs outside SSB slot(s) 229

A.3.2.2 Void 230

A.3.3 Reference DRX configurations 230

A.3.3.1 DRX Configuration 1: DRX cycle = 40 ms and TAT = 500 ms 230

A.3.3.2 DRX Configuration 2: DRX cycle = 640 ms and TAT = 500 ms 230

A.3.3.3 DRX Configuration 3: DRX cycle = 40 ms and TAT = Infinity 231

A.3.3.4 DRX Configuration 4: DRX cycle = 160 ms and TAT = Infinity 231

A.3.3.5 DRX Configuration 5: DRX cycle = 320 ms and TAT = Infinity 231

A.3.3.6 DRX Configuration 6: DRX cycle = 320 ms and TAT = 500 ms 232

A.3.3.7 DRX Configuration 7: DRX cycle = 640 ms and TAT = Infinity 232

A.3.3.8 DRX Configuration 8: DRX cycle = 320 ms and TAT = Infinity 232

A.3.3.9 DRX Configuration 9: DRX cycle = 40 ms and TAT = 500 ms 233

A.3.3.10 DRX Configuration 10: DRX cycle = 640 ms and TAT = 500 ms 233

A.3.3.11 DRX Configuration 11: DRX cycle = 20 ms and TAT = Infinity 233

A.3.3.12 DRX Configuration 12: DRX cycle = 640 ms and TAT = Infinity 234

A.3.4 Test Cases with Different Channel Bandwidths 234

A.3.4.1 Test Cases with Different E-UTRA Channel Bandwidths 234

A.3.4.1.1 Introduction 234

A.3.4.1.2 Principle of testing 234

A.3.5 Test Cases for Synchronous and Asynchronous DC Operations 234

A.3.5.1 EN-DC Test Cases for Synchronous and Asynchronous EN-DC Operations 234

A.3.5.1.1 Introduction 234

A.3.5.1.2 Principle of Testing 235

A.3.6 Antenna configurations 235

A.3.6.1 Antenna configurations for FR1 235

A.3.6.1.1 Antenna connection for 4 Rx capable UEs 235

A.3.6.1.1.1 Introduction 235

A.3.6.1.1.2 Principle of testing 235

A.3.6.2 Antenna configurations for FR2 238

A.3.7 EN-DC test setup 238

A.3.7.1 Introduction 238

A.3.7.2 E-UTRAN Serving Cell Parameters 238

A.3.7.2.1 E-UTRAN Serving Cell Parameters for Tests with NR Cell(s) in FR1 238

A.3.7.2.2 E-UTRAN Serving Cell Parameters for Tests with NR Cell(s) in FR2 239

A.3.7A NR FR1-FR2 test setup 240

A.3.7B Void 240

A.3.7C LTE-FR1/FR2 test setup 241

A.3.7D NE-DC test setup 241

A.3.7D.1 Introduction 241

A.3.7D.2 E-UTRAN Serving Cell Parameters 241

A.3.7D.2.1 E-UTRAN Serving Cell Parameters for Tests with NR Cell(s) in FR1 241

A.3.7D.2.2 E-UTRAN Serving Cell Parameters for Tests with NR Cell(s) in FR2 241

A.3.8 PRACH configurations 241

A.3.8.1 Introduction 241

A.3.8.2 PRACH configurations in FR1 241

A.3.8.2.1 FR1 PRACH configuration 1 241

A.3.8.2.2 FR1 PRACH configuration 2 242

A.3.8.2.3 FR1 PRACH configuration 3 243

A.3.8.2.4 FR1 PRACH configuration 4 244

A.3.8.3 PRACH configurations in FR2 245

A.3.8.3.1 FR2 PRACH configuration 1 245

A.3.8.3.2 FR2 PRACH configuration 2 246

A.3.8.3.3 FR2 PRACH configuration 3 247

A.3.8.3.4 FR2 PRACH configuration 4 248

A.3.9 BWP configurations 249

A.3.9.1 Introduction 249

A.3.9.2 Downlink BWP configurations 250

A.3.9.2.1 Initial BWP 250

A.3.9.2.2 Dedicated BWP 250

A.3.9.3 Uplink BWP configurations 250

A.3.9.3.1 Initial BWP 250

A.3.9.3.2 Dedicated BWP 251

A.3.10 SSB Configurations 251

A.3.10.1 SSB Configurations for FR1 251

A.3.10.1.1 SSB pattern 1 in FR1: SSB allocation for SSB SCS=15 kHz in 10 MHz 251

A.3.10.1.2 SSB pattern 2 in FR1: SSB allocation for SSB SCS=30 kHz in 40 MHz 252

A.3.10.1.3 SSB pattern 3 in FR1: SSB allocation for SSB SCS=15 kHz in 10 MHz 252

A.3.10.1.4 SSB pattern 4 in FR1: SSB allocation for SSB SCS=30 kHz in 40 MHz 253

A.3.10.1.5 SSB pattern 5 in FR1: SSB allocation for SSB SCS=15 kHz starting from odd SFN in 10 MHz 254

A.3.10.1.6 SSB pattern 6 in FR1: SSB allocation for SSB SCS=30 kHz starting from odd SFN in 40 MHz 254

A.3.10.2 SSB Configurations for FR2 255

A.3.10.2.1 SSB pattern 1 in FR2: SSB allocation for SSB SCS=120 kHz in 100 MHz 255

A.3.10.2.2 SSB pattern 2 in FR2: SSB allocation for SSB SCS=240 kHz in 100 MHz 255

A.3.10.2.3 SSB pattern 3 in FR2: SSB allocation for SSB SCS=120 kHz in 100 MHz 256

A.3.10.2.4 SSB pattern 4 in FR2: SSB allocation for SSB SCS=240 kHz in 100 MHz 256

A.3.10.2.5 SSB pattern 5 in FR2: SSB allocation for SSB SCS=120 kHz in 100 MHz 257

A.3.10.2.6 SSB pattern 6 in FR2: SSB allocation for SSB SCS=240 kHz in 100 MHz 257

A.3.10.2.7 SSB pattern 7 in FR2: SSB allocation for SSB SCS=120 kHz in 100 MHz 258

A.3.10.2.8 SSB pattern 8 in FR2: SSB allocation for SSB SCS=240 kHz in 100 MHz 258

A.3.11 SMTC Configurations 258

A.3.11.1 SMTC pattern 1: SMTC period = 20 ms with SMTC duration = 1 ms 258

A.3.11.2 SMTC pattern 2: SMTC period = 20 ms with SMTC duration = 5 ms 259

A.3.11.3 SMTC pattern 3: SMTC period = 160 ms with SMTC duration = 1 ms 259

A.3.11.4 SMTC pattern 4: SMTC period = 20 ms with SMTC duration = 1 ms 259

A.3.11.5 SMTC pattern 5: SMTC period = 20 ms with SMTC duration = 5 ms 259

A.3.11.6 SMTC pattern 6: SMTC period = 20 ms with SMTC duration = 5 ms 260

A.3.12 Test Cases with Different CC Configurations 260

A.3.12.1 EN-DC Test Cases with Different EN-DC Configurations 260

A.3.12.1.1 Introduction 260

A.3.12.1.2 Principle of testing 260

A.3.12.2 Carrier Aggregation Test Cases with Different CA Configurations 260

A.3.12.2.1 Introduction 260

A.3.12.2.2 Principle of testing 260

A.3.13 Test Cases in SA and EN-DC Operations 261

A.3.13.1 Introduction 261

A.3.13.2 Principle of Testing 261

A.3.13A Test Cases involving E-UTRA/FR1 and FR2 carriers 261

A.3.13A.1 Introduction 261

A.3.13A.2 Principle of Testing in EN-DC 261

A.3.13A.3 Principle of Testing in SA 262

A.3.13A.4 Principle of Testing in E-UTRA 262

A.3.13B Test Cases for EN-DC and NE-DC Operations 263

A.3.13B.1 Active BWP switch Test Cases for EN-DC and NE-DC Operations 263

A.3.13B.1.1 Introduction 263

A.3.13B.1.2 Principle of Testing 263

A.3.13B.2 SFTD accuracy Test Cases for EN-DC and NE-DC Operations 263

A.3.13B.2.1 Introduction 263

A.3.13B.2.2 Principle of Testing 263

A.3.14 CSI-RS configurations 263

A.3.14.1 FDD 263

A.3.14.2 TDD 264

A.3.15 Angle of Arrival (AoA) for FR2 RRM test cases 267

A.3.15.1 Setup 1: Single AoA in Rx beam peak direction 267

A.3.15.2 Setup 2: Single AoA in non Rx beam peak direction 267

A.3.15.2.1 Setup 2a: Single AoA in non Rx beam peak direction without change in direction 267

A.3.15.2.2 Setup 2b: Single AoA in non Rx beam peak direction with change in direction 267

A.3.15.3 Setup 3: 2 AoAs 267

A.3.15.4 Setup 4: 2 AoAs, 1 AoA in Rx beam peak direction, 1 in non Rx beam peak 268

A.3.15.4.1 Setup 4a: 2 AoAs, 1 AoA in Rx beam peak direction, 1 in non Rx beam peak without change in direction 268

A.3.15.4.2 Setup 4b: 2 AoAs, 1 AoA in Rx beam peak direction, 1 in non Rx beam peak with change in direction 268

A.3.16 TCI State Configuration 268

A.3.16.1 Introduction 268

A.3.16.2 TCI states 269

A.3.17 Configurations of CSI-RS for tracking 269

A.3.17.1 Configuration of CSI-RS for tracking for FR1 269

A.3.17.1.1 FDD 269

A.3.17.1.2 TDD 270

A.3.17.2 Configuration of CSI-RS for tracking for FR2 271

A.3.17.2.1 TDD 271

A.3.18 Additional definitions related to OTA testing for FR2 RRM test cases 272

A.3.18.1 Introduction 272

A.3.18.2 PRACH Power Measurement 272

A.4 EN-DC tests with all NR cells in FR1 273

A.4.1 Void 273

A.4.2 Void 273

A.4.3 RRC\_CONNECTED state mobility 273

A.4.3.1 Void 273

A.4.3.2 RRC Connection Mobility Control 273

A.4.3.2.1 Void 273

A.4.3.2.2 Random Access 273

A.4.3.2.2.1 Contention based random access test in FR1 for PSCell in EN-DC 273

A.4.3.2.2.1.1 Test Purpose and Environment 273

A.4.3.2.2.2 Non-contention based random access test in FR1 for PSCell in EN-DC 276

A.4.3.2.3 Void 279

A.4.4 Timing 279

A.4.4.1 UE transmit timing 279

A.4.4.1.1 NR UE Transmit Timing Test for FR1 279

A.4.4.1.1.1 Test Purpose and environment 279

A.4.4.1.1.2 Test requirements 282

A.4.4.2 UE timer accuracy 283

A.4.4.3 Timing advance 283

A.4.4.3.1 EN-DC FR1 timing advance adjustment accuracy 283

A.4.4.3.1.1 Test Purpose and Environment 283

A.4.4.3.1.2 Test Parameters 283

A.4.4.3.1.3 Test Requirements 286

A.4.5 Signaling characteristics 286

A.4.5.1 Radio link Monitoring 286

A.4.5.1.1 Radio Link Monitoring Out-of-sync Test for FR1 PSCell configured with SSB-based RLM RS in non-DRX mode 287

A.4.5.1.1.1 Test Purpose and Environment 287

A.4.5.1.1.2 Test Requirements 290

A.4.5.1.2 Radio Link Monitoring In-sync Test for FR1 PSCell configured with SSB-based RLM RS in non-DRX mode 290

A.4.5.1.2.2 Test Requirements 294

A.4.5.1.3 Radio Link Monitoring Out-of-sync Test for FR1 PSCell configured with SSB-based RLM RS in DRX mode 294

A.4.5.1.3.1 Test Purpose and Environment 294

A.4.5.1.3.2 Test Requirements 297

A.4.5.1.4 Radio Link Monitoring In-sync Test for FR1 PSCell configured with SSB-based RLM RS in DRX mode 298

A.4.5.1.4.1 Test Purpose and Environment 298

A.4.5.1.4.2 Test Requirements 301

A.4.5.1.5 EN-DC Radio Link Monitoring Out-of-sync Test for FR1 PSCell configured with CSI-RS-based RLM in non-DRX mode 302

A.4.5.1.5.1 Test Purpose and Environment 302

A.4.5.1.5.2 Test Requirements 305

A.4.5.1.6 EN-DC Radio Link Monitoring In-sync Test for FR1 PSCell configured with CSI-RS-based RLM in non-DRX mode 305

A.4.5.1.6.1 Test Purpose and Environment 305

A.4.5.1.6.2 Test Requirements 309

A.4.5.1.7 EN-DC Radio Link Monitoring Out-of-sync Test for FR1 PSCell configured with CSI-RS-based RLM in DRX mode 309

A.4.5.1.7.1 Test Purpose and Environment 309

A.4.5.1.7.2 Test Requirements 313

A.4.5.1.8 EN-DC Radio Link Monitoring In-sync Test for FR1 PSCell configured with CSI-RS-based RLM in DRX mode 313

A.4.5.1.8.1 Test Purpose and Environment 313

A.4.5.1.8.2 Test Requirements 317

A.4.5.2 Interruption 317

A.4.5.2.1 E-UTRAN – NR FR1 interruptions at transitions between active and non-active during DRX in synchronous EN-DC 317

A.4.5.2.1.1 Test Purpose and Environment 317

A.4.5.2.1.2 Test Requirements 320

A.4.5.2.2 E-UTRAN – NR FR1 interruptions at transitions between active and non-active during DRX in asynchronous EN-DC 320

A.4.5.2.2.1 Test Purpose and Environment 320

A.4.5.2.2.2 Test Requirements 323

A.4.5.2.3 E-UTRAN – NR FR1 interruptions during measurements on deactivated NR SCC in synchronous EN-DC 323

A.4.5.2.3.1 Test Purpose and Environment 323

A.4.5.2.3.2 Test Requirements 328

A.4.5.2.4 E-UTRAN – NR FR1 interruptions during measurements on deactivated NR SCC in asynchronous EN-DC 329

A.4.5.2.4.1 Test Purpose and Environment 329

A.4.5.2.4.2 Test Requirements 333

A.4.5.2.5 E-UTRAN – NR FR1 interruptions during measurements on deactivated E-UTRAN SCC in synchronous EN-DC 334

A.4.5.2.5.1 Test Purpose and Environment 334

A.4.5.2.5.2 Test Requirements 337

A.4.5.2.6 E-UTRAN – NR FR1 interruptions during measurements on deactivated E-UTRAN SCC in asynchronous EN-DC 337

A.4.5.2.6.1 Test Purpose and Environment 337

A.4.5.2.6.2 Test Requirements 340

A.4.5.2.7 Void 341

A.4.5.3.1 SCell Activation and deactivation of known SCell in FR1 for 160ms SCell measurement cycle 341

A.4.5.3.1.1 Test Purpose and Environment 341

A.4.5.3.1.2 Test Requirements 347

A.4.5.3.2 SCell Activation and deactivation of known SCell in FR1 for 640ms SCell measurement cycle 347

A.4.5.3.2.1 Test Purpose and Environment 347

A.4.5.3.2.2 Test Requirements 347

A.4.5.3.3 SCell Activation and deactivation of unknown SCell in FR1 348

A.4.5.3.3.1 Test Purpose and Environment 348

A.4.5.3.3.2 Test Requirements 349

A.4.5.4 UE UL carrier RRC reconfiguration Delay 349

A.4.5.4.1 UE UL carrier RRC reconfiguration Delay 349

A.4.5.4.1.1 Test Purpose and Environment 349

A.4.5.4.1.2 Test Requirements 355

A.4.5.5 Beam Failure Detection and Link recovery procedures 355

A.4.5.5.1 EN-DC Beam Failure Detection and Link Recovery Test for FR1 PSCell configured with SSB-based BFD and LR in non-DRX mode 355

A.4.5.5.1.1 Test Purpose and Environment 355

A.4.5.5.1.2 Test Requirements 361

A.4.5.5.2 EN-DC Beam Failure Detection and Link Recovery Test for FR1 PSCell configured with SSB-based BFD and LR in DRX mode 361

A.4.5.5.2.1 Test Purpose and Environment 361

A.4.5.5.2.2 Test Requirements 368

A.4.5.5.3 EN-DC Beam Failure Detection and Link Recovery Test for FR1 PSCell configured with CSI-RS-based BFD and LR in non-DRX mode 368

A.4.5.5.3.1 Test Purpose and Environment 368

A.4.5.5.3.2 Test Requirements 374

A.4.5.5.4 EN-DC Beam Failure Detection and Link Recovery Test for FR1 PSCell configured with CSI-RS-based BFD and LR in DRX mode 374

A.4.5.5.4.1 Test Purpose and Environment 374

A.4.5.5.4.2 Test Requirements 379

A.4.5.6.1 DCI-based and Timer-based Active BWP Switch 380

A.4.5.6.1.1 E-UTRAN – NR PSCell FR1 DL active BWP switch in non-DRX in synchronous EN-DC 380

A.4.5.6.1.1.1 Test Purpose and Environment 380

A.4.5.6.1.1.2 Test Requirements 383

A.4.5.6.1.2 E-UTRAN – NR PSCell FR1 DL active BWP switch with FR1 SCell in non-DRX in synchronous EN-DC 384

A.4.5.6.1.2.1 Test Purpose and Environment 384

A.4.5.6.1.2.2 Test Requirements 389

A.4.5.6.2 RRC-based Active BWP Switch 390

A.4.5.6.2.1.1 Test Purpose and Environment 390

A.4.5.6.2.1.2 Test Requirements 394

A.4.5.7 PSCell addition and release delay 395

A.4.5.7.1 Addition and Release Delay of known NR PSCell 395

A.4.5.7.1.1 Test purpose and environment 395

A.4.5.7.1.2 Test Requirements 398

A.4.6 Measurement procedure 399

A.4.6.1 Intra-frequency Measurements 399

A.4.6.1.1 EN-DC event triggered reporting tests without gap under non-DRX 399

A.4.6.1.1.1 Test purpose and Environment 399

A.4.6.1.1.2 Test parameters 399

A.4.6.1.1.3 Test Requirements 403

A.4.6.1.2 EN-DC event triggered reporting tests without gap under DRX 403

A.4.6.1.2.1 Test purpose and Environment 403

A.4.6.1.2.2 Test parameters 403

A.4.6.1.2.2 Test Requirements 407

A.4.6.1.3 EN-DC event triggered reporting tests with per-UE gaps under non-DRX 407

A.4.6.1.3.1 Test purpose and Environment 407

A.4.6.1.3.2 Test parameters 407

A.4.6.1.3.3 Test Requirements 411

A.4.6.1.4 EN-DC event triggered reporting tests with per-UE gaps under DRX 411

A.4.6.1.4.1 Test purpose and Environment 411

A.4.6.1.4.2 Test parameters 411

A.4.6.1.4.3 Test Requirements 415

A.4.6.1.5 EN-DC event triggered reporting tests without gap under non-DRX with SSB index reading 415

A.4.6.1.5.1 Test purpose and Environment 415

A.4.6.1.5.2 Test parameters 415

A.4.6.1.5.3 Test Requirements 417

A.4.6.1.6 EN-DC event triggered reporting tests with SSB index reading with per-UE gaps 418

A.4.6.1.6.1 Test purpose and Environment 418

A.4.6.1.6.2 Test parameters 418

A.4.6.1.6.3 Test Requirements 420

A.4.6.2 Inter-frequency Measurements 421

A.4.6.2.1 EN-DC event triggered reporting tests for FR1 cell without SSB time index detection when DRX is not used 421

A.4.6.2.1.1 Test Purpose and Environment 421

A.4.6.2.1.2 Test Requirements 424

A.4.6.2.2 EN-DC event triggered reporting tests for FR1 cell without SSB time index detection when DRX is used 424

A.4.6.2.2.1 Test Purpose and Environment 424

A.4.6.2.2.2 Test Requirements 428

A.4.6.2.3 Void 428

A.4.6.2.4 Void 428

A.4.6.2.5 EN-DC event triggered reporting tests for FR1 cell with SSB time index detection when DRX is not used 428

A.4.6.2.5.1 Test Purpose and Environment 428

A.4.6.2.5.2 Test Requirements 431

A.4.6.2.6 EN-DC event triggered reporting tests for FR1 cell with SSB time index detection when DRX is used 432

A.4.6.2.6.1 Test Purpose and Environment 432

A.4.6.2.6.2 Test Requirements 435

A.4.6.2.7 Void 436

A.4.6.2.8 Void 436

A.4.6.3 Void 436

A.4.6.4 L1-RSRP measurement for beam reporting 436

A.4.6.4.1 SSB based L1-RSRP measurement when DRX is not used 436

A.4.6.4.1.1 Test Purpose and Environment 436

A.4.6.4.1.2 Test parameters 436

A.4.6.4.1.3 Test Requirements 438

A.4.6.4.2 SSB based L1-RSRP measurement when DRX is used 438

A.4.6.4.2.1 Test Purpose and Environment 438

A.4.6.4.2.2 Test parameters 439

A.4.6.4.2.3 Test Requirements 441

A.4.6.4.3 CSI-RS based L1-RSRP measurement when DRX is not used 441

A.4.6.4.3.1 Test Purpose and Environment 441

A.4.6.4.3.2 Test parameters 442

A.4.6.4.3.3 Test Requirements 444

A.4.6.4.4 CSI-RS based L1-RSRP measurement when DRX is used 444

A.4.6.4.4.1 Test Purpose and Environment 444

A.4.6.4.4.2 Test parameters 444

A.4.6.4.4.3 Test Requirements 447

A.4.7 Measurement Performance requirements 447

A.4.7.1 SS-RSRP 448

A.4.7.1.1 EN-DC Intra-frequency measurement accuracy with FR1 serving cell and FR1 target cell 448

A.4.7.1.1.1 Test Purpose and Environment 448

A.4.7.1.1.2 Test parameters 448

A.4.7.1.1.3 Test Requirements 451

A.4.7.1.2 EN-DC inter-frequency measurement accuracy with FR1 serving cell and FR1 target cell 451

A.4.7.1.2.1 Test Purpose and Environment 451

A.4.7.1.2.2 Test parameters 451

A.4.7.1.2.3 Test Requirements 454

A.4.7.1.3 Void 454

A.4.7.2 SS-RSRQ 454

A.4.7.2.1 EN-DC Intra-frequency measurement accuracy with FR1 serving cell and FR1 target cell 454

A.4.7.2.1.1 Test Purpose and Environment 454

A.4.7.2.1.2 Test Parameters 454

A.4.7.2.1.3 Test Requirements 458

A.4.7.2.2 EN-DC Inter-frequency measurement accuracy with FR1 serving cell and FR1 target cell 458

A.4.7.2.2.1 Test Purpose and Environment 458

A.4.7.2.2.2 Test Parameters 458

A.4.7.2.2.3 Test Requirements 461

A.4.7.3 SS-SINR 462

A.4.7.3.1 EN-DC Intra-frequency measurement accuracy with FR1 serving cell and FR1 target cell 462

A.4.7.3.1.1 Test Purpose and Environment 462

A.4.7.3.1.2 Test Parameters 462

A.4.7.3.1.3 Test Requirements 465

A.4.7.3.2 EN-DC Inter-frequency measurement accuracy with FR1 serving cell and FR1 target cell 465

A.4.7.3.2.1 Test Purpose and Environment 465

A.4.7.3.2.2 Test Parameters 465

A.4.7.3.2.3 Test Requirements 469

A.4.7.4 L1-RSRP measurement for beam reporting 470

A.4.7.4.1 SSB based L1-RSRP measurement 470

A.4.7.4.1.1 Test Purpose and Environment 470

A.4.7.4.1.2 Test parameters 470

A.4.7.4.1.3 Test Requirements 473

A.4.7.4.2 CSI-RS based L1-RSRP measurement on resource set with repetition off 473

A.4.7.4.2.1 Test Purpose and Environment 473

A.4.7.4.2.2 Test parameters 473

A.4.7.4.2.3 Test Requirements 476

A.4.7.5 SFTD accuracy 476

A.4.7.5.1 SFTD accuracy 476

A.4.7.5.1.1 Test Purpose and Environment 476

A.4.7.5.1.2 Test Parameters 476

A.4.7.5.1.3 Test Requirements 479

A.4.7.5.2 Void 479

A.4.7.5.3 Void 479

A.4.8 Void 479

A.4A NE-DC test with all NR cells in FR1 480

A.4A.1 Signaling characteristics 480

A.4A.1.1 E-UTRAN PSCell addition 480

A.4A.1.1.1 Test purpose and environment 480

A.4A.1.1.2 Test Requirements 484

A.4A.1.2 Active BWP switch 485

A.4A.1.2.1 E-UTRAN PSCell – NR PCell FR1 DCI-based and Timer-based DL active BWP switch in non-DRX in synchronous NE-DC 485

A.4A.1.2.1.1 Test Purpose and Environment 485

A.4A.2 Measurement performance 490

A.4A.2.1 SFTD accuracy 490

A.4A.2.1.1 SFTD accuracy 490

A.4A.2.1.1.1 Test Purpose 490

A.4A.2.1.1.2 Test Environment 490

A.4A.2.1.1.3 Test Requirements 493

A.5 EN-DC tests with one or more NR cells in FR2 494

A.5.1 Void 494

A.5.2 Void 494

A.5.3 RRC\_CONNECTED state mobility 494

A.5.3.1 Void 494

A.5.3.2 RRC Connection Mobility Control 494

A.5.3.2.1 Void 494

A.5.3.2.2 Random Access 494

A.5.3.2.2.1 Contention based random access test in FR2 for PSCell/SCell in EN-DC 494

A.5.3.2.2.2 Non-contention based random access test in FR2 for PSCell/SCell in EN-DC 498

A.5.3.2.3 Void 503

A.5.4 Timing 503

A.5.4.1 UE transmit timing 503

A.5.4.1.1 NR UE Transmit Timing Test for FR2 503

A.5.4.1.1.1 Test Purpose and environment 503

A.5.4.1.1.2 Test requirements 506

A.5.4.2 UE timer accuracy 506

A.5.4.3 Timing advance 506

A.5.4.3.1 EN-DC FR2 timing advance adjustment accuracy 506

A.5.4.3.1.1 Test Purpose and Environment 506

A.5.4.3.1.2 Test Parameters 507

A.5.4.3.1.3 Test Requirements 510

A.5.5 Signaling characteristics 510

A.5.5.1 Radio link Monitoring 510

A.5.5.1.1 Radio Link Monitoring Out-of-sync Test for FR2 PSCell configured with SSB-based RLM RS in non-DRX mode 510

A.5.5.1.1.1 Test Purpose and Environment 510

A.5.5.1.1.2 Test Requirements 514

A.5.5.1.2 Radio Link Monitoring In-sync Test for FR2 PSCell configured with SSB-based RLM RS in non-DRX mode 515

A.5.5.1.2.1 Test Purpose and Environment 515

A.5.5.1.2.2 Test Requirements 518

A.5.5.1.3 Radio Link Monitoring Out-of-sync Test for FR2 PSCell configured with SSB-based RLM RS in DRX mode 518

A.5.5.1.3.1 Test Purpose and Environment 518

A.5.5.1.3.2 Test Requirements 523

A.5.5.1.4 Radio Link Monitoring In-sync Test for FR2 PSCell configured with SSB-based RLM RS in DRX mode 523

A.5.5.1.4.1 Test Purpose and Environment 523

A.5.5.1.4.2 Test Requirements 527

A.5.5.1.5 EN-DC Radio Link Monitoring Out-of-sync Test for FR2 PSCell configured with CSI-RS-based RLM in non-DRX mode 527

A.5.5.1.6 EN-DC Radio Link Monitoring In-sync Test for FR2 PSCell configured with CSI-RS-based RLM in non-DRX mode 531

A.5.5.1.6.1 Test Purpose and Environment 531

A.5.5.1.6.2 Test Requirements 535

A.5.5.1.7 EN-DC Radio Link Monitoring Out-of-sync Test for FR2 PSCell configured with CSI-RS-based RLM in DRX mode 535

A.5.5.1.7.1 Test Purpose and Environment 535

A.5.5.1.7.2 Test Requirements 540

A.5.5.1.8 EN-DC Radio Link Monitoring In-sync Test for FR2 PSCell configured with CSI-RS-based RLM in DRX mode 540

A.5.5.1.8.1 Test Purpose and Environment 540

A.5.5.1.8.2 Test Requirements 544

A.5.5.1.9 EN-DC Radio Link Monitoring UE Scheduling Restrictions on FR2 545

A.5.5.1.9.1 Test Purpose and Environment 545

A.5.5.1.9.2 Test Requirements 547

A.5.5.2 Interruption 547

A.5.5.2.1 E-UTRAN – NR FR2 interruptions at transitions between active and non-active during DRX in synchronous EN-DC 547

A.5.5.2.1.1 Test Purpose and Environment 547

A.5.5.2.1.2 Test Requirements 550

A.5.5.2.2 E-UTRAN – NR FR2 interruptions at transitions between active and non-active during DRX in asynchronous EN-DC 550

A.5.5.2.2.1 Test Purpose and Environment 550

A.5.5.2.2.2 Test Requirements 553

A.5.5.2.3 E-UTRAN – NR FR2 interruptions during measurements on deactivated NR SCC in synchronous EN-DC 553

A.5.5.2.3.1 Test Purpose and Environment 553

A.5.5.2.3.2 Test Requirements 556

A.5.5.2.4 E-UTRAN – NR FR2 interruptions during measurements on deactivated NR SCC in asynchronous EN-DC 557

A.5.5.2.4.1 Test Purpose and Environment 557

A.5.5.2.4.2 Test Requirements 560

A.5.5.2.5 E-UTRAN – NR FR2 interruptions during measurements on deactivated E-UTRAN SCC in synchronous EN-DC 561

A.5.5.2.5.1 Test Purpose and Environment 561

A.5.5.2.5.2 Test Requirements 564

A.5.5.2.6 E-UTRAN – NR FR2 interruptions during measurements on deactivated E-UTRAN SCC in asynchronous EN-DC 565

A.5.5.2.6.1 Test Purpose and Environment 565

A.5.5.2.6.2 Test Requirements 567

A.5.5.3.1 SCell Activation and deactivation of SCell in FR2 intra-band 568

A.5.5.3.1.1 Test Purpose and Environment 568

A.5.5.3.1.2 Test Requirements 570

A.5.5.3.2 SCell Activation and deactivation of known SCell in FR1 for 160ms SCell measurement cycle 570

A.5.5.3.2.1 Test Purpose and Environment 570

A.5.5.3.2.2 Test Requirements 573

A.5.5.3.3 Void 573

A.5.5.3.4 Void 573

A.5.5.3.5 SCell Activation and deactivation of SCell in FR2 573

A.5.5.3.5.1 Test Purpose and Environment 573

A.5.5.3.5.2 Test Requirements 576

A.5.5.4 Void 577

A.5.5.5 Beam Failure Detection and Link recovery procedures 577

A.5.5.5.1 EN-DC Beam Failure Detection and Link Recovery Test for FR2 PSCell configured with SSB-based BFD and LR in non-DRX mode 577

A.5.5.5.1.1 Test Purpose and Environment 577

A.5.5.5.1.2 Test Requirements 581

A.5.5.5.2 EN-DC Beam Failure Detection and Link Recovery Test for FR2 PSCell configured with SSB-based BFD and LR in DRX mode 581

A.5.5.5.2.1 Test Purpose and Environment 581

A.5.5.5.2.2 Test Requirements 585

A.5.5.5.3 EN-DC Beam Failure Detection and Link Recovery Test for FR2 PSCell configured with CSI-RS-based BFD and LR in non-DRX mode 585

A.5.5.5.3.1 Test Purpose and Environment 585

A.5.5.5.3.2 Test Requirements 589

A.5.5.5.4 EN-DC Beam Failure Detection and Link Recovery Test for FR2 PSCell configured with CSI-RS-based BFD and LR in DRX mode 589

A.5.5.5.4.1 Test Purpose and Environment 589

A.5.5.5.4.2 Test Requirements 593

A.5.5.5.5 EN-DC scheduling availability restriction during Beam Failure Detection and Link Recovery for FR2 PSCell configured with SSB-based BFD and LR in non-DRX mode 593

A.5.5.5.5.1 Test Purpose and Environment 593

A.5.5.5.5.2 Test Requirements 597

A.5.5.6 Active BWP switch 597

A.5.5.6.1 DCI-based and Timer-based Active BWP Switch 597

A.5.5.6.1.1 E-UTRAN – NR PSCell FR2 DL active BWP switch with non-DRX in synchronous EN-DC 597

A.5.5.6.1.1.1 Test Purpose and Environment 597

A.5.5.6.1.1.2 Test Requirements 601

A.5.5.6.1.2 E-UTRAN – NR PSCell FR2 with FR2 SCell DL active BWP switch in non-DRX in synchronous EN-DC 602

A.5.5.6.1.2.1 Test Purpose and Environment 602

A.5.5.6.1.2.2 Test Requirements 605

A.5.5.6.2 RRC-based Active BWP Switch 606

A.5.5.6.2.1 E-UTRAN – NR PSCell FR2 DL active BWP switch with non-DRX in synchronous EN-DC 606

A.5.5.6.2.1.1 Test Purpose and Environment 606

A.5.5.6.2.1.2 Test Requirements 609

A.5.5.7 PSCell addition and release delay 610

A.5.5.7.1 Addition and Release Delay of NR PSCell 610

A.5.5.7.1.1 Test purpose and environment 610

A.5.5.7.1.2 Test Requirements 613

A.5.5.8 Active TCI state switch delay 614

A.5.5.8.1 MAC-CE based active TCI state switch 614

A.5.5.8.1.1 E-UTRAN – NR PSCell FR2 active TCI state switch for a known TCI state 614

A.5.5.8.1.1.1 Test Purpose and Environment 614

A.5.5.8.1.1.2 Test Requirements 617

A.5.5.8.2 RRC based active TCI state switch 617

A.5.5.8.2.1 E-UTRAN – NR PSCell FR2 active TCI state switch for a known TCI state 617

A.5.5.8.2.1.1 Test Purpose and Environment 617

A.5.5.8.2.1.2 Test Requirements 621

A.5.6 Measurement procedure 621

A.5.6.1 Intra-frequency Measurements 621

A.5.6.1.1 EN-DC event triggered reporting test without gap under non-DRX 621

A.5.6.1.1.1 Test purpose and Environment 621

A.5.6.1.1.2 Test Requirements 625

A.5.6.1.2 EN-DC event triggered reporting test without gap under DRX 625

A.5.6.1.2.1 Test purpose and Environment 625

A.5.6.1.2.2 Test Requirements 627

A.5.6.1.3 EN-DC event triggered reporting test with per-UE gaps under non-DRX 628

A.5.6.1.3.1 Test purpose and Environment 628

A.5.6.1.3.2 Test Requirements 632

A.5.6.1.4 EN-DC event triggered reporting test with per-UE gaps under DRX 632

A.5.6.1.4.1 Test purpose and Environment 632

A.5.6.1.4.2 Test Requirements 635

A.5.6.2 Inter-frequency Measurements 636

A.5.6.2.1 EN-DC event triggered reporting tests for FR2 cell without SSB time index detection when DRX is not used 636

A.5.6.2.1.1 Test Purpose and Environment 636

A.5.6.2.1.2 Test Requirements 639

A.5.6.2.2 EN-DC event triggered reporting tests for FR2 cell without SSB time index detection when DRX is used 639

A.5.6.2.2.1 Test Purpose and Environment 639

A.5.6.2.2.2 Test Requirements 642

A.5.6.2.3 EN-DC event triggered reporting tests for FR2 cell with SSB time index detection when DRX is not used 642

A.5.6.2.3.1 Test Purpose and Environment 642

A.5.6.2.3.2 Test Requirements 646

A.5.6.2.4 EN-DC event triggered reporting tests for FR2 cell with SSB time index detection when DRX is used 646

A.5.6.2.4.1 Test Purpose and Environment 646

A.5.6.2.5 EN-DC event triggered reporting tests for FR2 cell without SSB time index detection when DRX is not used 650

A.5.6.2.5.1 Test Purpose and Environment 650

A.5.6.2.5.2 Test Requirements 653

A.5.6.2.6 EN-DC event triggered reporting tests for FR2 cell without SSB time index detection when DRX is used 654

A.5.6.2.6.1 Test Purpose and Environment 654

A.5.6.2.6.2 Test Requirements 658

A.5.6.2.7 EN-DC event triggered reporting tests for FR2 cell with SSB time index detection when DRX is not used 658

A.5.6.2.7.1 Test Purpose and Environment 658

A.5.6.2.7.2 Test Requirements 662

A.5.6.2.8 EN-DC event triggered reporting tests for FR2 cell with SSB time index detection when DRX is used 663

A.5.6.2.8.1 Test Purpose and Environment 663

A.5.6.2.8.2 Test Requirements 667

A.5.6.3 L1-RSRP measurement for beam reporting 668

A.5.6.3.1 SSB based L1-RSRP measurement when DRX is not used 668

A.5.6.3.1.1 Test Purpose and Environment 668

A.5.6.3.1.2 Test parameters 668

A.5.6.3.1.3 Test Requirements 670

A.5.6.3.1.3 Test Requirements 670

A.5.6.3.2 SSB based L1-RSRP measurement when DRX is used 671

A.5.6.3.2.1 Test Purpose and Environment 671

A.5.6.3.2.2 Test parameters 671

A.5.6.3.2.3 Test Requirements 673

A.5.6.3.3 CSI-RS based L1-RSRP measurement when DRX is not used 673

A.5.6.3.3.1 Test Purpose and Environment 673

A.5.6.3.3.2 Test parameters 674

A.5.6.3.3.3 Test Requirements 675

A.5.6.3.4 CSI-RS based L1-RSRP measurement when DRX is used 676

A.5.6.3.4.1 Test Purpose and Environment 676

A.5.6.3.4.2 Test parameters 676

A.5.6.3.4.3 Test Requirements 678

A.5.7 Measurement Performance requirements 679

A.5.7.1 SS-RSRP 679

A.5.7.1.1 EN-DC intra-frequency case measurement accuracy with FR2 serving cell and FR2 target cell 679

A.5.7.1.1.1 Test Purpose and Environment 679

A.5.7.1.1.2 Test parameters 679

A.5.7.1.1.3 Test Requirements 681

A.5.7.1.2 EN-DC inter-frequency case measurement accuracy with FR2 serving cell and FR2 target cell 682

A.5.7.1.2.1 Test Purpose and Environment 682

A.5.7.1.2.2 Test parameters 682

A.5.7.1.2.3 Test Requirements 687

A.5.7.1.3 EN-DC inter-frequency measurement accuracy with FR1 serving cell and FR2 target cell 688

A.5.7.1.3.1 Test Purpose and Environment 688

A.5.7.1.3.2 Test parameters 688

A.5.7.1.3.3 Test Requirements 691

A.5.7.2 SS-RSRQ 691

A.5.7.2.1 EN-DC Intra-frequency measurement accuracy with FR2 serving cell and FR2 TDD target cell 691

A.5.7.2.1.1 Test Purpose and Environment 691

A.5.7.2.1.2 Test Parameters 691

A.5.7.2.1.3 Test Requirements 693

A.5.7.2.2 EN-DC Inter-frequency measurement accuracy with FR2 serving cell and FR2 TDD target cell 693

A.5.7.2.2.1 Test Purpose and Environment 693

A.5.7.2.2.2 Test Parameters 694

A.5.7.2.2.3 Test Requirements 696

A.5.7.3 SS-SINR 696

A.5.7.3.1 EN-DC Intra-frequency measurement accuracy with FR2 serving cell and FR2 TDD target cell 696

A.5.7.3.1.1 Test Purpose and Environment 696

A.5.7.3.1.2 Test Parameters 697

A.5.7.3.1.3 Test Requirements 699

A.5.7.3.2 EN-DC Inter-frequency measurement accuracy with FR2 serving cell and FR2 TDD target cell 700

A.5.7.3.2.1 Test Purpose and Environment 700

A.5.7.3.2.2 Test Parameters 700

A.5.7.3.2.3 Test Requirements 702

A.5.7.4 L1-RSRP measurement for beam reporting 702

A.5.7.4.1 SSB based L1-RSRP measurement 702

A.5.7.4.1.1 Test Purpose and Environment 702

A.5.7.4.1.2 Test parameters 703

A.5.7.4.1.3 Test Requirements 705

A.5.7.4.2 CSI-RS based L1-RSRP measurement on resource set with repetition off 706

A.5.7.4.2.1 Test Purpose and Environment 706

A.5.7.4.2.2 Test parameters 706

A.5.7.4.2.3 Test Requirements 708

A.5.8 Void 709

A.6 NR standalone tests with all NR cells in FR1 674

A.6.1 SA: RRC\_IDLE state mobility 674

A.6.1.1 Cell re-selection to NR 674

A.6.1.1.1 Cell reselection to FR1 intra-frequency NR case 674

A.6.1.1.1.1 Test Purpose and Environment 674

A.6.1.1.1.2 Test Parameters 674

A.6.1.1.1.3 Test Requirements 678

A.6.1.1.2 Cell reselection to FR1 inter-frequency NR case 678

A.6.1.1.2.1 Test Purpose and Environment 678

A.6.1.1.2.2 Test Parameters 678

A.6.1.1.2.3 Test Requirements 682

A.6.1.2.1 Cell reselection to higher priority E-UTRAN 682

A.6.1.2.1.1 Test Purpose and Environment 682

A.6.1.2.1.2 Test Parameters 682

A.6.1.2.1.3 Test Requirements 685

A.6.1.2.2 Cell reselection to lower priority E-UTRAN 686

A.6.1.2.2.1 Test Purpose and Environment 686

A.6.1.2.2.2 Test Parameters 686

A.6.1.2.2.3 Test Requirements 688

A.6.2 SA: RRC\_INACTIVE state mobility 689

A.6.3 RRC\_CONNECTED state mobility 689

A.6.3.1.1 Intra-frequency handover from FR1 to FR1; known target cell 689

A.6.3.1.1.1 Test Purpose and Environment 689

A.6.3.1.1.2 Test Parameters 689

A.6.3.1.1.3 Test Requirements 691

A.6.3.1.2 Intra-frequency handover from FR1 to FR1; unknown target cell 691

A.6.3.1.2.1 Test Purpose and Environment 691

A.6.3.1.2.2 Test Parameters 691

A.6.3.1.2.3 Test Requirements 693

A.6.3.1.3 Inter-frequency handover from FR1 to FR1; unknown target cell 693

A.6.3.1.3.1 Test Purpose and Environment 693

A.6.3.1.3.2 Test Parameters 693

A.6.3.1.3.3 Test Requirements 695

A.6.3.1.4 SA NR - E-UTRAN handover 695

A.6.3.1.4.1 Test Purpose and Environment 695

A.6.3.1.4.2 Test Requirements 699

A.6.3.1.5 SA NR - E-UTRAN handover with unknown target cell 699

A.6.3.1.5.1 Test Purpose and Environment 699

A.6.3.1.5.2 Test Requirements 702

A.6.3.2.1 SA: RRC Re-establishment 703

A.6.3.2.1.1 Intra-frequency RRC Re-establishment in FR1 703

A.6.3.2.1.2 Inter-frequency RRC Re-establishment in FR1 706

A.6.3.2.1.3 Intra-frequency RRC Re-establishment in FR1 without serving cell timing 709

A.6.3.2.2 Random Access 712

A.6.3.2.2.1 Contention based random access test in FR1 for NR standalone 712

A.6.3.2.2.2 Non-Contention based random access test in FR1 for NR standalone 716

A.6.3.2.3.1 Redirection from NR in FR1 to NR in FR1 719

A.6.3.2.3.2 Redirection from NR in FR1 to E-UTRAN 722

A.6.4 Timing 726

A.6.4.1.1 NR UE Transmit Timing Test for FR1 726

A.6.4.1.1.1 Test Purpose and environment 726

A.6.4.1.1.2 Test requirements 728

A.6.4.3.1 SA FR1 timing advance adjustment accuracy 729

A.6.4.3.1.1 Test Purpose and Environment 729

A.6.4.3.1.2 Test Parameters 729

A.6.4.3.1.3 Test Requirements 732

A.6.5 Signalling characteristics 732

A.6.5.1.1 Radio Link Monitoring Out-of-sync Test for FR1 PCell configured with SSB-based RLM RS in non-DRX mode 733

A.6.5.1.1.1 Test Purpose and Environment 733

A.6.5.1.1.2 Test Requirements 736

A.6.5.1.2 Radio Link Monitoring In-sync Test for FR1 PCell configured with SSB-based RLM RS in non-DRX mode 736

A.6.5.1.2.1 Test Purpose and Environment 736

A.6.5.1.2.2 Test Requirements 740

A.6.5.1.3 Radio Link Monitoring Out-of-sync Test for FR1 PCell configured with SSB-based RLM RS in DRX mode 740

A.6.5.1.3.1 Test Purpose and Environment 740

A.6.5.1.3.2 Test Requirements 744

A.6.5.1.4 Radio Link Monitoring In-sync Test for FR1 PCell configured with SSB-based RLM RS in DRX mode 744

A.6.5.1.4.1 Test Purpose and Environment 744

A.6.5.1.4.2 Test Requirements 748

A.6.5.1.5 Radio Link Monitoring Out-of-sync Test for FR1 PCell configured with CSI-RS-based RLM in non-DRX mode 748

A.6.5.1.5.1 Test Purpose and Environment 748

A.6.5.1.5.2 Test Requirements 753

A.6.5.1.6 Radio Link Monitoring In-sync Test for FR1 PCell configured with CSI-RS-based RLM in non-DRX mode 753

A.6.5.1.6.1 Test Purpose and Environment 753

A.6.5.1.6.2 Test Requirements 757

A.6.5.1.7 Radio Link Monitoring Out-of-sync Test for FR1 PCell configured with CSI-RS-based RLM in DRX mode 757

A.6.5.1.7.1 Test Purpose and Environment 757

A.6.5.1.7.2 Test Requirements 761

A.6.5.1.8 Radio Link Monitoring In-sync Test for FR1 PCell configured with CSI-RS-based RLM in DRX mode 761

A.6.5.1.8.1 Test Purpose and Environment 761

A.6.5.1.8.2 Test Requirements 765

A.6.5.2.1 Interruptions during measurements on deactivated NR SCC in FR1 765

A.6.5.3.1 SCell Activation and deactivation of known SCell in FR1 in non-DRX for 160ms SCell measurement cycle 770

A.6.5.3.1.1 Test Purpose and Environment 770

A.6.5.3.1.2 Test Requirements 775

A.6.5.3.2 SCell Activation and deactivation of known SCell in FR1 in non-DRX for 640 ms SCell measurement cycle 776

A.6.5.3.2.1 Test Purpose and Environment 776

A.6.5.3.2.2 Test Requirements 776

A.6.5.3.3 SCell Activation and deactivation of unknown SCell in FR1 in non-DRX 776

A.6.5.3.3.1 Test Purpose and Environment 776

A.6.5.3.3.2 Test Requirements 777

A.6.5.4.1 UE UL carrier RRC reconfiguration Delay 777

A.6.5.4.1.1 Test Purpose and Environment 777

A.6.5.4.1.2 Test Requirements 784

A.6.5.4.2 Void 785

A.6.5.5.1 Beam Failure Detection and Link Recovery Test for FR1 PCell configured with SSB-based BFD and LR in non-DRX mode 785

A.6.5.5.1.1 Test Purpose and Environment 785

A.6.5.5.1.2 Test Requirements 789

A.6.5.5.2 Beam Failure Detection and Link Recovery Test for FR1 PCell configured with SSB-based BFD and LR in DRX mode 789

A.6.5.5.2.1 Test Purpose and Environment 789

A.6.5.5.2.2 Test Requirements 794

A.6.5.5.3 Beam Failure Detection and Link Recovery Test for FR1 PCell configured with CSI-RS-based BFD and LR in non-DRX mode 794

A.6.5.5.3.1 Test Purpose and Environment 794

A.6.5.5.3.2 Test Requirements 800

A.6.5.5.4 Beam Failure Detection and Link Recovery Test for FR1 PCell configured with CSI-RS-based BFD and LR in DRX mode 800

A.6.5.5.4.1 Test Purpose and Environment 800

A.6.5.5.4.2 Test Requirements 805

A.6.5.6.1 DCI-based and Timer-based Active BWP Switch 805

A.6.5.6.1.1 NR FR1- NR FR1 DL active BWP switch of SCell with non-DRX in SA 805

A.6.5.6.1.2 NR FR1 DL active BWP switch with non-DRX in SA 812

A.6.5.6.2 RRC-based Active BWP Switch 816

A.6.5.6.2.1 NR FR1 DL active BWP switch of Cell with non-DRX in SA 816

A.6.6 Measurement procedure 819

A.6.6.1.1 SA event triggered reporting tests without gap under non-DRX 819

A.6.6.1.1.1 Test purpose and Environment 819

A.6.6.1.1.2 Test parameters 819

A.6.6.1.1.3 Test Requirements 821

A.6.6.1.2 SA event triggered reporting tests without gap under DRX 821

A.6.6.1.2.1 Test purpose and Environment 821

A.6.6.1.2.2 Test parameters 822

A.6.6.1.2.3 Test Requirements 823

A.6.6.1.3 SA event triggered reporting tests with per-UE gaps under non-DRX 824

A.6.6.1.3.1 Test purpose and Environment 824

A.6.6.1.3.2 Test parameters 824

A.6.6.1.3.3 Test Requirements 828

A.6.6.1.4 SA event triggered reporting tests with per-UE gaps under DRX 828

A.6.6.1.4.1 Test purpose and Environment 828

A.6.6.1.4.2 Test parameters 828

A.6.6.1.4.3 Test Requirements 831

A.6.6.1.5 SA event triggered reporting tests without gap under non-DRX with SSB index reading 831

A.6.6.1.5.1 Test purpose and Environment 831

A.6.6.1.5.2 Test parameters 831

A.6.6.1.5.3 Test Requirements 833

A.6.6.1.6 SA event triggered reporting tests with per-UE gaps under non-DRX with SSB index reading 833

A.6.6.1.6.1 Test purpose and Environment 833

A.6.6.1.6.2 Test parameters 833

A.6.6.1.6.3 Test Requirements 835

A.6.6.2.1 SA event triggered reporting tests for FR1 without SSB time index detection when DRX is not used 835

A.6.6.2.1.1 Test Purpose and Environment 835

A.6.6.2.1.2 Test Requirements 838

A.6.6.2.2 SA event triggered reporting tests for FR1 without SSB time index detection when DRX is used 838

A.6.6.2.2.1 Test Purpose and Environment 838

A.6.6.2.2.2 Test Requirements 841

A.6.6.2.3 Void 842

A.6.6.2.4 Void 842

A.6.6.2.5 SA event triggered reporting tests for FR1 with SSB time index detection when DRX is not used 842

A.6.6.2.5.1 Test Purpose and Environment 842

A.6.6.2.5.2 Test Requirements 846

A.6.6.2.6 SA event triggered reporting tests for FR1 with SSB time index detection when DRX is used 846

A.6.6.2.6.1 Test Purpose and Environment 846

A.6.6.2.6.2 Test Requirements 849

A.6.6.2.7 Void 850

A.6.6.2.8 Void 850

A.6.6.3 Inter-RAT Measurements 850

A.6.6.3.1 SA NR - E-UTRAN event-triggered reporting in non-DRX in FR1 850

A.6.6.3.1.1 Test Purpose and Environment 850

A.6.6.3.1.2 Test Requirements 853

A.6.6.3.2 SA NR - E-UTRAN event-triggered reporting in DRX in FR1 854

A.6.6.3.2.1 Test Purpose and Environment 854

A.6.6.3.2.2 Test Requirements 857

A.6.6.4 L1-RSRP measurement for beam reporting 858

A.6.6.4.1 SSB based L1-RSRP measurement when DRX is not used 858

A.6.6.4.1.1 Test Purpose and Environment 858

A.6.6.4.1.2 Test parameters 858

A.6.6.4.1.3 Test Requirements 860

A.6.6.4.2 SSB based L1-RSRP measurement when DRX is used 860

A.6.6.4.2.1 Test Purpose and Environment 860

A.6.6.4.2.2 Test parameters 860

A.6.6.4.2.3 Test Requirements 863

A.6.6.4.3 CSI-RS based L1-RSRP measurement when DRX is not used 863

A.6.6.4.3.1 Test Purpose and Environment 863

A.6.6.4.3.2 Test parameters 863

A.6.6.4.3.3 Test Requirements 865

A.6.6.4.4 CSI-RS based L1-RSRP measurement when DRX is used 865

A.6.6.4.4.1 Test Purpose and Environment 865

A.6.6.4.4.2 Test parameters 865

A.6.6.4.4.3 Test Requirements 867

A.6.7 Measurement Performance requirements 868

A.6.7.1.1 SA: intra-frequency case measurement accuracy with FR1 serving cell and FR1 target cell 868

A.6.7.1.1.1 Test Purpose and Environment 868

A.6.7.1.1.2 Test parameters 868

A.6.7.1.1.3 Test Requirements 873

A.6.7.1.2 SA inter-frequency case measurement accuracy with FR1 serving cell and FR1 target cell 873

A.6.7.1.2.1 Test Purpose and Environment 873

A.6.7.1.2.2 Test parameters 873

A.6.7.1.2.3 Test Requirements 876

A.6.7.1.3 Void 876

A.6.7.2 SS-RSRQ 876

A.6.7.2.1 SA: Intra-frequency measurement accuracy with FR1 serving cell and FR1 target cell 876

A.6.7.2.1.1 Test Purpose and Environment 876

A.6.7.2.1.2 Test Parameters 876

A.6.7.2.1.3 Test Requirements 880

A.6.7.2.2 SA Inter-frequency measurement accuracy with FR1 serving cell and FR1 target cell 880

A.6.7.2.2.1 Test Purpose and Environment 880

A.6.7.2.2.2 Test Parameters 880

A.6.7.2.2.3 Test Requirements 884

A.6.7.3.1 SA intra-frequency measurement accuracy with FR1 serving cell and FR1 target cell 884

A.6.7.3.1.1 Test Purpose and Environment 884

A.6.7.3.1.2 Test Parameters 884

A.6.7.3.1.3 Test Requirements 887

A.6.7.3.2 SA Inter-frequency measurement accuracy with FR1 serving cell and FR1 target cell 888

A.6.7.3.2.1 Test Purpose and Environment 888

A.6.7.3.2.2 Test Parameters 888

A.6.7.3.2.3 Test Requirements 891

A.6.7.4.1 SSB based L1-RSRP measurement 891

A.6.7.4.1.1 Test Purpose and Environment 891

A.6.7.4.1.2 Test parameters 891

A.6.7.4.1.3 Test Requirements 894

A.6.7.4.2 CSI-RS based L1-RSRP measurement on resource set with repetition off 894

A.6.7.4.2.1 Test Purpose and Environment 894

A.6.7.4.2.2 Test parameters 894

A.6.7.4.2.3 Test Requirements 897

A.6.7.5.1 SA: inter-RAT measurement accuracy with FR1 serving cell 897

A.6.7.5.1.1 Test Purpose and Environment 897

A.6.7.5.1.2 Test parameters 897

A.6.7.5.1.3 Test Requirements 902

A.6.7.6.1 SA: inter-RAT measurement accuracy with FR1 serving cell 903

A.6.7.6.1.1 Test Purpose and Environment 903

A.6.7.6.1.2 Test parameters 903

A.6.7.6.1.3 Test Requirements 908

A.6.7.7.1 SA: inter-RAT measurement accuracy with FR1 serving cell 908

A.6.7.7.1.1 Test Purpose and Environment 908

A.6.7.7.1.2 Test parameters 908

A.6.7.7.1.3 Test Requirements 913

A.7 NR standalone tests with one or more NR cells in FR2 913

A.7.1 SA: RRC\_IDLE state mobility 913

A.7.1.1.1 Cell reselection to FR2 intra-frequency NR case 913

A.7.1.1.1.1 Test Purpose and Environment 913

A.7.1.1.1.2 Test Parameters 913

A.7.1.1.1.3 Test Requirements 916

A.7.1.1.2 Cell reselection to FR2 inter-frequency NR case 916

A.7.1.1.2.1 Test Purpose and Environment 916

A.7.1.1.2.2 Test Parameters 917

A.7.1.1.2.3 Test Requirements 919

A.7.2 SA: RRC\_INACTIVE state mobility 919

A.7.3 RRC\_CONNECTED state mobility 919

A.7.3.1 Handover 919

A.7.3.1.1 Inter-frequency handover from FR1 to FR2; unknown target cell 919

A.7.3.1.1.1 Test Purpose and Environment 919

A.7.3.1.1.2 Test Parameters 919

A.7.3.1.1.3 Test Requirements 922

A.7.3.1.2 Intra-frequency handover from FR2 to FR2; unknown target cell 923

A.7.3.1.2.1 Test Purpose and Environment 923

A.7.3.1.2.2 Test Parameters 923

A.7.3.1.2.3 Test Requirements 925

A.7.3.1.3 Inter-frequency handover from FR2 to FR2; unknown target cell 925

A.7.3.1.3.1 Test Purpose and Environment 925

A.7.3.1.3.2 Test Parameters 925

A.7.3.1.3.3 Test Requirements 927

A.7.3.2.1 SA: RRC Re-establishment 927

A.7.3.2.1.1 Intra-frequency RRC Re-establishment in FR2 927

A.7.3.2.1.2 Inter-frequency RRC Re-establishment in FR2 930

A.7.3.2.1.3 Intra-frequency RRC Re-establishment in FR2 without serving cell timing 933

A.7.3.2.1.3.1 Test Purpose and Environment 933

A.7.3.2.1.3.2 Test Requirements 935

A.7.3.2.2 Random Access 936

A.7.3.2.2.1 Contention based random access test in FR2 for NR Standalone 936

A.7.3.2.2.2 Non-contention based random access test in FR2 for NR Standalone 940

A.7.3.2.3 SA: RRC Connection Release with Redirection 944

A.7.3.2.3.1 Redirection from NR in FR2 to NR in FR2 944

A.7.4 Timing 946

A.7.4.1.1 NR UE Transmit Timing Test for FR2 946

A.7.4.1.1.1 Test Purpose and environment 946

A.7.4.1.1.2 Test requirements 949

A.7.4.3.1 SA FR2 timing advance adjustment accuracy 950

A.7.4.3.1.1 Test Purpose and Environment 950

A.7.4.3.1.2 Test Parameters 950

A.7.4.3.1.3 Test Requirements 954

A.7.5 Signaling characteristics 954

A.7.5.1.1 Radio Link Monitoring Out-of-sync Test for FR2 PCell configured with SSB-based RLM RS in non-DRX mode 954

A.7.5.1.1.1 Test Purpose and Environment 954

A.7.5.1.1.2 Test Requirements 957

A.7.5.1.2 Radio Link Monitoring In-sync Test for FR2 PCell configured with SSB-based RLM RS in non-DRX mode 958

A.7.5.1.2.1 Test Purpose and Environment 958

A.7.5.1.2.2 Test Requirements 962

A.7.5.1.3 Radio Link Monitoring Out-of-sync Test for FR2 PCell configured with SSB-based RLM RS in DRX mode 963

A.7.5.1.3.1 Test Purpose and Environment 963

A.7.5.1.3.2 Test Requirements 967

A.7.5.1.4 Radio Link Monitoring In-sync Test for FR2 PCell configured with SSB-based RLM RS in DRX mode 967

A.7.5.1.4.1 Test Purpose and Environment 967

A.7.5.1.4.2 Test Requirements 972

A.7.5.1.5 Radio Link Monitoring Out-of-sync Test for FR2 PCell configured with CSI-RS-based RLM in non-DRX mode 972

A.7.5.1.5.1 Test Purpose and Environment 972

A.7.5.1.5.2 Test Requirements 977

A.7.5.1.6 Radio Link Monitoring In-sync Test for FR2 PCell configured with CSI-RS-based RLM in non-DRX mode 977

A.7.5.1.6.1 Test Purpose and Environment 977

A.7.5.1.6.2 Test Requirements 981

A.7.5.1.7 Radio Link Monitoring Out-of-sync Test for FR2 PCell configured with CSI-RS-based RLM in DRX mode 981

A.7.5.1.7.1 Test Purpose and Environment 981

A.7.5.1.7.2 Test Requirements 985

A.7.5.1.8 Radio Link Monitoring In-sync Test for FR2 PCell configured with CSI-RS-based RLM in DRX mode 985

A.7.5.1.8.1 Test Purpose and Environment 985

A.7.5.1.8.2 Test Requirements 990

A.7.5.1.9 UE Radio Link Monitoring Scheduling Restrictions on FR2 990

A.7.5.1.9.1 Test Purpose and Environment 990

A.7.5.1.9.2 Test Requirements 993

A.7.5.2.1 Interruptions during measurements on deactivated NR SCC in FR2 993

A.7.5.3.1 SCell Activation and deactivation for SCell in FR2 intra-band in non-DRX 997

A.7.5.3.1.1 Test Purpose and Environment 997

A.7.5.3.1.2 Test Requirements 999

A.7.5.3.2 SCell Activation and deactivation for FR1+FR2 inter-band with target SCell in FR2 999

A.7.5.3.2.1 Test Purpose and Environment 999

A.7.5.3.2.2 Test Requirements 1003

A.7.5.5.1 Beam Failure Detection and Link Recovery Test for FR2 PCell configured with SSB-based BFD and LR in non-DRX mode 1004

A.7.5.5.1.1 Test Purpose and Environment 1004

A.7.5.5.1.2 Test Requirements 1008

A.7.5.5.2 Beam Failure Detection and Link Recovery Test for FR2 PCell configured with SSB-based BFD and LR in DRX mode 1008

A.7.5.5.2.1 Test Purpose and Environment 1008

A.7.5.5.2.2 Test Requirements 1012

A.7.5.5.3 Beam Failure Detection and Link Recovery Test for FR2 PCell configured with CSI-RS-based BFD and LR in non-DRX mode 1012

A.7.5.5.3.1 Test Purpose and Environment 1012

A.7.5.5.3.2 Test Requirements 1015

A.7.5.5.4 Beam Failure Detection and Link Recovery Test for FR2 PCell configured with CSI-RS-based BFD and LR in DRX mode 1016

A.7.5.5.4.1 Test Purpose and Environment 1016

A.7.5.5.4.2 Test Requirements 1019

A.7.5.5.5 Scheduling availability restriction during Beam Failure Detection and Link Recovery for FR2 PCell configured with SSB-based BFD and LR in non-DRX mode 1020

A.7.5.5.5.1 Test Purpose and Environment 1020

A.7.5.5.5.2 Test Requirements 1024

A.7.5.6.1 DCI-based and Timer-based Active BWP Switch 1024

A.7.5.6.1.1 NR FR2- NR FR2 DL active BWP switch of SCell with non-DRX in SA 1024

A.7.5.6.1.2 NR FR1- NR FR2 DL active BWP switch of SCell with non-DRX in SA 1029

A.7.5.6.1.3 NR FR2 DL active BWP switch with non-DRX in SA 1033

A.7.5.6.1.3.1 Test Purpose and Environment 1033

A.7.5.6.1.3.2 Test Requirements 1036

A.7.5.6.2 RRC-based Active BWP Switch 1036

A.7.5.7.1 Addition and Release Delay of known NR PSCell 1040

A.7.5.7.1.1 Test Purpose and Environment 1040

A.7.5.7.2 Addition and Release Delay of unknown NR PSCell 1043

A.7.5.7.2.1 Test Purpose and Environment 1043

A.7.5.8.1 MAC-CE based active TCI state switch 1046

A.7.5.8.2 RRC based active TCI state switch 1050

A.7.6 Measurement procedure 1054

A.7.6.1.1 SA event triggered reporting test without gap under non-DRX 1054

A.7.6.1.1.1 Test purpose and Environment 1054

A.7.6.1.1.2 Test Requirements 1057

A.7.6.1.2 SA event triggered reporting test without gap under DRX 1058

A.7.6.1.2.1 Test purpose and Environment 1058

A.7.6.1.2.2 Test Requirements 1061

A.7.6.1.3 SA event triggered reporting test with per-UE gaps under non-DRX 1061

A.7.6.1.3.1 Test purpose and Environment 1061

A.7.6.1.3.2 Test Requirements 1064

A.7.6.1.4 SA event triggered reporting test with per-UE gaps under DRX 1065

A.7.6.1.4.1 Test purpose and Environment 1065

A.7.6.1.4.2 Test Requirements 1068

A.7.6.2.1 SA event triggered reporting tests For FR2 without SSB time index detection when DRX is not used (PCell in FR2) 1068

A.7.6.2.1.1 Test Purpose and Environment 1068

A.7.6.2.1.2 Test Requirements 1072

A.7.6.2.2 SA event triggered reporting tests For FR2 without SSB time index detection when DRX is used (PCell in FR2) 1072

A.7.6.2.2.1 Test Purpose and Environment 1072

A.7.6.2.2.2 Test Requirements 1075

A.7.6.2.3 SA event triggered reporting tests For FR2 with SSB time index detection when DRX is not used (PCell in FR2) 1075

A.7.6.2.3.1 Test Purpose and Environment 1075

A.7.6.2.3.2 Test Requirements 1079

A.7.6.2.4 SA event triggered reporting tests For FR2 with SSB time index detection when DRX is used (PCell in FR2) 1079

A.7.6.2.4.1 Test Purpose and Environment 1079

A.7.6.2.4.2 Test Requirements 1082

A.7.6.2.5 SA event triggered reporting tests for FR2 without SSB time index detection when DRX is not used (PCell in FR1) 1082

A.7.6.2.5.1 Test Purpose and Environment 1082

A.7.6.2.5.2 Test Requirements 1085

A.7.6.2.6 SA event triggered reporting tests for FR2 without SSB time index detection when DRX is used (PCell in FR1) 1086

A.7.6.2.6.1 Test Purpose and Environment 1086

A.7.6.2.6.2 Test Requirements 1089

A.7.6.2.7 SA event triggered reporting tests for FR2 with SSB time index detection when DRX is not used (PCell in FR1) 1090

A.7.6.2.7.1 Test Purpose and Environment 1090

A.7.6.2.7.2 Test Requirements 1093

A.7.6.2.8 SA event triggered reporting tests for FR2 with SSB time index detection when DRX is used (PCell in FR1) 1093

A.7.6.2.8.1 Test Purpose and Environment 1093

A.7.6.2.8.2 Test Requirements 1097

A.7.6.3 L1-RSRP measurement for beam reporting 1098

A.7.6.3.1 SSB based L1-RSRP measurement when DRX is not used 1098

A.7.6.3.1.1 Test Purpose and Environment 1098

A.7.6.3.1.2 Test parameters 1098

A.7.6.3.1.3 Test Requirements 1100

A.7.6.3.2 SSB based L1-RSRP measurement when DRX is used 1100

A.7.6.3.2.1 Test Purpose and Environment 1100

A.7.6.3.2.2 Test parameters 1101

A.7.6.3.2.3 Test Requirements 1103

A.7.6.3.3 CSI-RS based L1-RSRP measurement when DRX is not used 1103

A.7.6.3.3.1 Test Purpose and Environment 1103

A.7.6.3.3.2 Test parameters 1104

A.7.6.3.3.3 Test Requirements 1106

A.7.6.3.4 CSI-RS based L1-RSRP measurement when DRX is used 1107

A.7.6.3.4.1 Test Purpose and Environment 1107

A.7.6.3.4.2 Test parameters 1107

A.7.6.3.4.3 Test Requirements 1109

A.7.7 Measurement Performance requirements 1110

A.7.7.1.1 SA intra-frequency case measurement accuracy with FR2 serving cell and FR2 target cell 1110

A.7.7.1.1.1 Test Purpose and Environment 1110

A.7.7.1.1.2 Test parameters 1110

A.7.7.1.1.3 Test Requirements 1113

A.7.7.1.2 SA inter-frequency case measurement accuracy with FR2 serving cell and FR2 target cell 1113

A.7.7.1.2.1 Test Purpose and Environment 1113

A.7.7.1.2.2 Test parameters 1114

A.7.7.1.2.3 Test Requirements 1118

A.7.7.1.3 SA inter-frequency measurement accuracy with FR1 serving cell and FR2 target cell 1119

A.7.7.1.3.1 Test Purpose and Environment 1119

A.7.7.1.3.2 Test parameters 1119

A.7.7.1.3.3 Test Requirements 1121

A.7.7.2 SS-RSRQ 1122

A.7.7.2.1 SA intra-frequency measurement accuracy with FR2 serving cell and FR2 target cell 1122

A.7.7.2.1.1 Test Purpose and Environment 1122

A.7.7.2.1.2 Test Parameters 1122

A.7.7.2.1.3 Test Requirements 1124

A.7.7.2.2 SA Inter-frequency measurement accuracy with FR2 serving cell and FR2 TDD target cell 1124

A.7.7.2.2.1 Test Purpose and Environment 1124

A.7.7.2.2.2 Test Parameters 1124

A.7.7.2.2.3 Test Requirements 1126

A.7.7.3.1 SA intra-frequency case measurement accuracy with FR2 serving cell and FR2 target cell 1126

A.7.7.3.1.1 Test Purpose and Environment 1126

A.7.7.3.1.2 Test Parameters 1127

A.7.7.3.1.3 Test Requirements 1128

A.7.7.3.2 SA Inter-frequency measurement accuracy with FR2 serving cell and FR2 TDD target cell 1128

A.7.7.3.2.1 Test Purpose and Environment 1128

A.7.7.3.2.2 Test Parameters 1128

A.7.7.3.2.3 Test Requirements 1130

A.7.7.4.1 SSB based L1-RSRP measurement 1130

A.7.7.4.1.1 Test Purpose and Environment 1130

A.7.7.4.1.2 Test parameters 1131

A.7.7.4.1.3 Test Requirements 1133

A.7.7.4.2 CSI-RS based L1-RSRP measurement on resource set with repetition off 1134

A.7.7.4.2.1 Test Purpose and Environment 1134

A.7.7.4.2.2 Test parameters 1134

A.7.7.4.2.3 Test Requirements 1136

A.8 E-UTRA standalone tests for NR RRM 1137

A.8.1 Void 1137

A.8.2 RRC\_IDLE state mobility 1137

A.8.2.1 Inter-RAT NR Cell re-selection 1137

A.8.2.1.1 E-UTRA Cell reselection to higher priority NR target Cell in FR1 1137

A.8.2.1.1.1 Test Purpose and Environment 1137

A.8.2.1.1.2 Test Requirements 1140

A.8.3 RRC\_CONNECTED state mobility 1141

A.8.3.1 Handover 1141

A.8.3.1.1 E-UTRAN - NR handover in FR1 1141

A.8.3.1.1.1 Test Purpose and Environment 1141

A.8.3.1.1.2 Test Requirements 1146

A.8.4 Measurement procedure 1146

A.8.4.1.1 E-UTRA – NR Inter-RAT SFTD Measurement Delay in non-DRX 1146

A.8.4.1.1.1 Test Purpose and Environment 1146

A.8.4.1.1.2 Test Requirements 1148

A.8.4.1.2 E-UTRA – NR Inter-RAT SFTD Measurement Delay in DRX 1149

A.8.4.1.2.1 Test Purpose and Environment 1149

A.8.4.1.2.2 Test Requirements 1150

A.8.4.2 E-UTRA – NR Inter-RAT Measurements 1150

A.8.4.2.1 NR Inter-RAT event triggered reporting tests for FR1 without SSB time index detection when DRX is not used 1150

A.8.4.2.1.1 Test Purpose and Environment 1150

A.8.4.2.1.2 Test Requirements 1154

A.8.4.2.2 NR Inter-RAT event triggered reporting tests for FR1 without SSB time index detection when DRX is used 1155

A.8.4.2.2.1 Test Purpose and Environment 1155

A.8.4.2.2.2 Test Requirements 1158

A.8.4.2.3 NR Inter-RAT event triggered reporting tests for FR1 with SSB time index detection when DRX is not used 1159

A.8.4.2.3.1 Test Purpose and Environment 1159

A.8.4.2.3.2 Test Requirements 1162

A.8.4.2.4 NR Inter-RAT event triggered reporting tests for FR1 with SSB time index detection when DRX is used 1163

A.8.4.2.4.1 Test Purpose and Environment 1163

A.8.4.2.4.2 Test Requirements 1168

A.8.4.2.5 NR Inter-RAT event triggered reporting tests for FR2 without SSB time index detection when DRX is not used 1169

A.8.4.2.5.1 Test Purpose and Environment 1169

A.8.4.2.5.2 Test Requirements 1171

A.8.4.2.6 NR Inter-RAT event triggered reporting tests for FR2 without SSB time index detection when DRX is used 1172

A.8.4.2.6.1 Test Purpose and Environment 1172

A.8.4.2.6.2 Test Requirements 1174

A.8.4.2.7 NR Inter-RAT event triggered reporting tests for FR2 with SSB time index detection when DRX is not used 1175

A.8.4.2.7.1 Test Purpose and Environment 1175

A.8.4.2.7.2 Test Requirements 1177

A.8.4.2.8 NR Inter-RAT event triggered reporting tests for FR2 with SSB time index detection when DRX is used 1178

A.8.4.2.8.1 Test Purpose and Environment 1178

A.8.4.2.8.2 Test Requirements 1180

A.8.5 Measurement performance 1181

A.8.5.1.1 SFTD accuracy 1181

A.8.5.1.1.1 Test Purpose 1181

A.8.5.1.1.2 Test Environment 1181

A.8.5.1.1.3 Test Requirements 1185

A.8.5.2 E-UTRA – NR Inter-RAT Measurement Performance requirements 1185

A.8.5.2.1 SS-RSRP 1185

A.8.5.2.1.1 E-UTRAN – NR inter-RAT measurements with FR1 target cell 1185

A.8.5.2.1.2 E-UTRAN – NR inter-RAT measurements with FR2 target cell 1189

A.8.5.2.1.2.1 Test Purpose and Environment 1189

A.8.5.2.1.2.2 Test Parameters 1189

A.8.5.2.1.2.3 Test Requirements 1191

A.8.5.2.2 SS-RSRQ 1192

A.8.5.2.2.1 E-UTRAN – NR inter-RAT measurements with FR1 target cell 1192

A.8.5.2.2.2 E-UTRAN – NR inter-RAT measurements with FR2 target cell 1195

A.8.5.2.2.2.1 Test Purpose and Environment 1195

A.8.5.2.2.2.2 Test Parameters 1195

A.8.5.2.2.2.3 Test Requirements 1197

A.8.5.2.3 SS-SINR 1198

A.8.5.2.3.1 E-UTRAN – NR inter-RAT measurements with FR1 target cell 1198

A.8.5.2.3.2 E-UTRAN – NR inter-RAT measurements with FR2 target cell 1201

A.8.5.2.3.2.1 Test Purpose and Environment 1201

A.8.5.2.3.2.2 Test Parameters 1201

A.8.5.2.3.2.3 Test Requirements 1202

Annex B (normative): Conditions for RRM requirements applicability for operating bands 1186

B.1 Conditions for NR RRC\_IDLE state mobility 1186

B.1.1 Introduction 1186

B.1.2 Conditions for measurements on NR intra-frequency cells for cell re-selection 1186

B.1.3 Conditions for measurements on NR inter-frequency cells for cell re-selection 1187

B.2 Conditions for UE measurements procedures and performance requirements in RRC\_CONNECTED state 1188

B.2.1 Introduction 1188

B.2.1.1 General 1188

B.2.1.2 Derivation of Minimum SSB\_RP values for FR1 1188

B.2.1.3 Derivation of Minimum SSB\_RP values for FR2 1188

B.2.1.3.1 Minimum SSB\_RP values for Rx Beam Peak angle of arrival 1188

B.2.1.4 Gain to SS-RSRP measurement point for FR1 1190

B.2.1.5 Gain to SS-RSRP measurement point for FR2 1190

B.2.1.5.1 Gain to SS-RSRP measurement point for Rx Beam Peak angle of arrival 1190

B.2.1.5.2 Gain to SS-RSRP measurement point for different frequency 1190

B.2.1.5.3 Alignment of Rough beam to Rx beam Peak 1191

B.2.2 Conditions for NR intra-frequency measurements 1191

B.2.3 Conditions for NR inter-frequency measurements 1192

B.2.4 Conditions for NR L1-RSRP reporting 1193

B.2.4.1 Conditions for SSB based L1-RSRP reporting 1193

B.2.4.2 Conditions for CSI-RS based L1-RSRP reporting 1194

B.2.5 Conditions for RRC connection release with redirection to NR 1196

B.2.6 Void 1197

B.2.6.1 Void 1197

B.2.6.2 Void 1197

B.3 RRM Requirements Exceptions 1197

B.3.1 Introduction 1197

B.3.2 Receiver sensitivity relaxation for CA 1197

B.3.2.1 Receiver sensitivity relaxation for UE supporting CA in FR1 1197

B.3.2.2 Receiver sensitivity relaxation for UE configured with CA in FR1 1197

B.3.2.2.1 Inter-band carrier aggregation 1197

B.3.2.2.2 Reference sensitivity exceptions due to UL harmonic interference for CA 1197

B.3.2.2.3 Reference sensitivity exceptions due to intermodulation interference due to 2UL CA 1198

B.3.2.3 Receiver sensitivity relaxation for UE supporting CA in FR2 1198

B.3.2.4 Receiver sensitivity relaxation for UE configured with CA in FR2 1198

B.3.2.4.1 Intra-band contiguous carrier aggregation 1198

B.3.2.4.2 Intra-band non-contiguous carrier aggregation 1198

B.3.3 Receiver sensitivity relaxation for DC 1198

B.3.3.1 Receiver sensitivity relaxation for EN-DC 1198

B.3.3.2 Receiver sensitivity relaxation for NE-DC 1198

B.3.4 Receiver sensitivity relaxation for SUL 1198

B.3.4.1 Receiver sensitivity relaxation for UE supporting SUL in FR1 1198

B.3.4.2 Receiver sensitivity relaxation for UE configured with SUL in FR1 1198

B.3.4.2.1 Reference sensitivity exceptions due to UL harmonic interference for SUL 1198

Annex C (informative): Change history 1200