3GPP TS 36.213 V15.16.0 (2022-09)

Technical Specification

3rd Generation Partnership Project;

Technical Specification Group Radio Access Network;

Evolved Universal Terrestrial Radio Access (E-UTRA);

Physical layer procedures

(Release 15)

** 

The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP.  
The present document has not been subject to any approval process by the 3GPPOrganisational Partners and shall not be implemented.  
This Specification is provided for future development work within 3GPPonly. The Organisational Partners accept no liability for any use of this Specification.  
Specifications and reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organisational Partners' Publications Offices.

Keywords

E-UTRA, radio, layer 1

***3GPP***

Postal address

3GPP support office address

650 Route des Lucioles – Sophia Antipolis

Valbonne – France

Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16

Internet

http://www.3gpp.org

***Copyright Notification***

No part may be reproduced except as authorized by written permission.  
The copyright and the foregoing restriction extend to reproduction in all media.

© 2022, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

UMTS™ is a Trade Mark of ETSI registered for the benefit of its members

3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  
LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners

GSM® and the GSM logo are registered and owned by the GSM Association

Contents

Foreword 8

1 Scope 9

2 References 9

3 Symbols and abbreviations 10

3.1 Symbols 10

3.2 Abbreviations 10

4 Synchronization procedures 12

4.1 Cell search 12

4.2 Timing synchronization 12

4.2.1 Radio link monitoring 12

4.2.2 Inter-cell synchronization 12

4.2.3 Transmission timing adjustments 12

4.3 Timing for Secondary Cell Activation / Deactivation 14

5 Power control 15

5.1 Uplink power control 15

5.1.1 Physical uplink shared channel 15

5.1.1.1 UE behaviour 16

5.1.1.2 Power headroom 30

5.1.2 Physical uplink control channel 33

5.1.2.1 UE behaviour 34

5.1.3 Sounding Reference Symbol (SRS) 39

5.1.3.1 UE behaviour 39

5.1.3.2 Power headroom for Type3 report 41

5.1.4 Power allocation for EUTRA dual connectivity 42

5.1.4.1 Dual connectivity power control Mode 1 43

5.1.4.2 Dual connectivity power control Mode 2 50

5.1.5 Power allocation for PUCCH-SCell 54

5.2 Downlink power allocation 55

5.2.1 eNodeB Relative Narrowband TX Power (RNTP) restrictions 58

6 Random access procedure 59

6.1 Physical non-synchronized random access procedure 59

6.1.1 Timing 60

6.2 Random Access Response Grant 61

7 Physical downlink shared channel related procedures 66

7.1 UE procedure for receiving the physical downlink shared channel 67

7.1.1 Single-antenna port scheme 86

7.1.2 Transmit diversity scheme 86

7.1.3 Large delay CDD scheme 86

7.1.4 Closed-loop spatial multiplexing scheme 86

7.1.5 Multi-user MIMO scheme 87

7.1.5A Dual layer scheme 87

7.1.5B Up to 8 layer transmission scheme 87

7.1.6 Resource allocation 87

7.1.6.1 Resource allocation type 0 89

7.1.6.2 Resource allocation type 1 90

7.1.6.3 Resource allocation type 2 91

7.1.6.4 PDSCH starting position 94

7.1.6.4A PDSCH starting position for BL/CE UEs 96

7.1.6.5 Physical Resource Block (PRB) bundling 96

7.1.7 Modulation order and transport block size determination 98

7.1.7.1 Modulation order and redundancy version determination 100

7.1.7.2 Transport block size determination 106

7.1.7.2.1 Transport blocks not mapped to two or more layer spatial multiplexing 111

7.1.7.2.2 Transport blocks mapped to two-layer spatial multiplexing 119

7.1.7.2.3 Transport blocks mapped for DCI Format 1C and DCI Format 6-2 119

7.1.7.2.4 Transport blocks mapped to three-layer spatial multiplexing 120

7.1.7.2.5 Transport blocks mapped to four-layer spatial multiplexing 120

7.1.7.2.6 Transport blocks mapped for BL/CE UEs configured with CEModeB and PDSCH bandwidth up to 1.4MHz 121

7.1.7.2.7 Transport blocks mapped for BL/CE UEs *SystemInformationBlockType1-BR* 122

7.1.7.2.8 Transport blocks mapped for UEs configured with *ce-pdsch-maxBandwidth-config* value of 5 MHz or with *pdsch-MaxBandwidth-SC-MTCH* value of 24 PRBs 122

7.1.7.3 Redundancy Version determination for Format 1C 122

7.1.8 Storing soft channel bits 123

7.1.9 PDSCH resource mapping parameters 123

7.1.10 Antenna ports quasi co-location for PDSCH 125

7.1.11 PDSCH subframe assignment for BL/CE UE 126

7.2 UE procedure for reporting Channel State Information (CSI) 128

7.2.1 Aperiodic CSI Reporting using PUSCH 138

7.2.2 Periodic CSI Reporting using PUCCH 164

7.2.3 Channel Quality Indicator (CQI) definition 204

7.2.4 Precoding Matrix Indicator (PMI) definition 218

7.2.5 Channel-State Information – Reference Signal (CSI-RS) definition 246

7.2.6 Channel-State Information – Interference Measurement (CSI-IM) Resource definition 248

7.2.7 Zero Power CSI-RS Resource definition 248

7.2.8 CSI-RS Activation / Deactivation 248

7.3 UE procedure for reporting HARQ-ACK 249

7.3.1 FDD HARQ-ACK reporting procedure 251

7.3.2 TDD HARQ-ACK reporting procedure 256

7.3.2.1 TDD HARQ-ACK reporting procedure for same UL/DL configuration 257

7.3.2.2 TDD HARQ-ACK reporting procedure for different UL/DL configurations 272

7.3.3 FDD-TDD HARQ-ACK reporting procedure for primary cell frame structure type 1 279

7.3.4 FDD-TDD HARQ-ACK reporting procedure for primary cell frame structure type 2 281

8 Physical uplink shared channel related procedures 283

8.0 UE procedure for transmitting the physical uplink shared channel 283

8.0.1 Single-antenna port scheme 309

8.0.2 Closed-loop spatial multiplexing scheme 309

8.1 Resource allocation for PDCCH/EPDCCH/SPDCCH with uplink DCI format 310

8.1.1 Uplink resource allocation type 0 310

8.1.2 Uplink resource allocation type 1 311

8.1.3 Uplink resource allocation type 2 311

8.1.4 Uplink resource allocation type 3 312

8.1.5 Uplink resource allocation type 4 313

8.1.5.1 UL Resource Block Groups 313

8.1.6 Uplink resource allocation type 5 314

8.2 UE sounding procedure 316

8.3 UE HARQ-ACK procedure 327

8.3A Autonomous uplink feedback procedure 329

8.4 UE PUSCH hopping procedure 329

8.4.1 Type 1 PUSCH hopping 330

8.4.2 Type 2 PUSCH hopping 330

8.5 UE Reference Symbol (RS) procedure 331

8.6 Modulation order, redundancy version and transport block size determination 332

8.6.1 Modulation order and redundancy version determination 332

8.6.2 Transport block size determination 340

8.6.3 Control information MCS offset determination 346

8.7 UE transmit antenna selection 350

8.8 Transmission timing adjustments 350

9 Physical downlink control channel procedures 350

9.1 UE procedure for determining physical downlink control channel assignment 351

9.1.1 PDCCH assignment procedure 351

9.1.2 PHICH assignment procedure 355

9.1.3 Control Format Indicator (CFI) assignment procedure 358

9.1.4 EPDCCH assignment procedure 359

9.1.4.1 EPDCCH starting position 366

9.1.4.2 Antenna ports quasi co-location for EPDCCH 366

9.1.4.3 Resource mapping parameters for EPDCCH 367

9.1.4.4 PRB-pair indication for EPDCCH 367

9.1.5 MPDCCH assignment procedure 368

9.1.5.1 MPDCCH starting position 375

9.1.5.2 Antenna ports quasi co-location for MPDCCH 375

9.1.6 SPDCCH assignment procedure 375

9.1.6.1 Resource mapping parameters for SPDCCH 377

9.1.6.2 PRB-pair indication for SPDCCH 377

9.1.6.3 Physical Resource Block (PRB) bundling for DMRS-based SPDCCH 378

9.1.6.4 Antenna ports quasi co-location for DMRS-based SPDCCH 378

9.2 PDCCH/EPDCCH/MPDCCH/SPDCCH validation for semi-persistent scheduling 379

9.2A PDCCH/EPDCCH validation for autonomous uplink transmissions 381

9.3 PDCCH/EPDCCH/MPDCCH/SPDCCH control information procedure 382

10 Physical uplink control channel procedures 383

10.1 UE procedure for determining physical uplink control channel assignment 384

10.1.1 PUCCH format information 389

10.1.2 FDD HARQ-ACK feedback procedures 395

10.1.2.1 FDD HARQ-ACK procedure for one configured serving cell 395

10.1.2.2 FDD HARQ-ACK procedures for more than one configured serving cell 399

10.1.2.2.1 PUCCH format 1b with channel selection HARQ-ACK procedure 399

10.1.2.2.2 PUCCH format 3 HARQ-ACK procedure 403

10.1.2.2.3 PUCCH format 4 HARQ-ACK procedure 405

10.1.2.2.4 PUCCH format 5 HARQ-ACK procedure 408

10.1.3 TDD HARQ-ACK feedback procedures 409

10.1.3.1 TDD HARQ-ACK procedure for one configured serving cell 411

10.1.3.2 TDD HARQ-ACK procedure for more than one configured serving cell 425

10.1.3.2.1 PUCCH format 1b with channel selection HARQ-ACK procedure 425

10.1.3.2.2 PUCCH format 3 HARQ-ACK procedure 441

10.1.3.2.3 PUCCH format 4 HARQ-ACK procedure 448

10.1.3.2.4 PUCCH format 5 HARQ-ACK procedure 465

10.1.3A FDD-TDD HARQ-ACK feedback procedures for primary cell frame structure type 2 465

10.1.4 HARQ-ACK Repetition procedure 467

10.1.5 Scheduling Request (SR) procedure 468

10.2 Uplink HARQ-ACK timing 470

11 Physical Multicast Channel (PMCH) related procedures 475

11.1 UE procedure for receiving the PMCH 475

11.2 UE procedure for receiving MCCH and system information change notification 476

12 Assumptions independent of physical channel 476

13 Uplink/Downlink configuration determination procedure for Frame Structure Type 2 476

13.1 UE procedure for determining eIMTA-uplink/downlink configuration 477

13A Subframe configuration for Frame Structure Type 3 478

14 UE procedures related to Sidelink 481

14.1 Physical Sidelink Shared Channel related procedures 482

14.1.1 UE procedure for transmitting the PSSCH 482

14.1.1.1 UE procedure for determining subframes for transmitting PSSCH for sidelink transmission mode 1 484

14.1.1.1.1 Determination of subframe indicator bitmap 484

14.1.1.2 UE procedure for determining resource blocks for transmitting PSSCH for sidelink transmission mode 1 487

14.1.1.2.1 PSSCH resource allocation for sidelink transmission mode 1 487

14.1.1.2.2 PSSCH frequency hopping for sidelink transmission mode 1 488

14.1.1.3 UE procedure for determining subframes for transmitting PSSCH for sidelink transmission mode 2 488

14.1.1.4 UE procedure for determining resource blocks for transmitting PSSCH for sidelink transmission mode 2 489

14.1.1.4A UE procedure for determining subframes and resource blocks for transmitting PSSCH for sidelink transmission mode 3 489

14.1.1.4B UE procedure for determining subframes and resource blocks for transmitting PSSCH and reserving resources for sidelink transmission mode 4 490

14.1.1.4C UE procedure for determining subframes and resource blocks for PSSCH transmission associated with an SCI format 1 490

14.1.1.5 UE procedure for PSSCH power control 491

14.1.1.6 UE procedure for determining the subset of resources to be reported to higher layers in PSSCH resource selection in sidelink transmission mode 4 and in sensing measurement in sidelink transmission mode 3 493

14.1.1.7 Conditions for selecting resources when the number of HARQ transmissions is two in sidelink transmission mode 4 496

14.1.2 UE procedure for receiving the PSSCH 496

14.1.3 UE procedure for determining resource block pool and subframe pool for sidelink transmission mode 2 497

14.1.5 UE procedure for determining resource block pool and subframe pool for sidelink transmission mode 3 and 4 498

14.2 Physical Sidelink Control Channel related procedures 499

14.2.1 UE procedure for transmitting the PSCCH 499

14.2.1.1 UE procedure for determining subframes and resource blocks for transmitting PSCCH for sidelink transmission mode 1 502

14.2.1.2 UE procedure for determining subframes and resource blocks for transmitting PSCCH for sidelink transmission mode 2 502

14.2.1.3 UE procedure for PSCCH power control 502

14.2.2 UE procedure for receiving the PSCCH 504

14.2.3 UE procedure for determining resource block pool and subframe pool for PSCCH 504

14.2.4 UE procedure for determining resource block pool for PSCCH in sidelink transmission mode 3 and 4 505

15 Void 508

16 UE Procedures related to narrowband IoT 508

16.1 Synchronization procedures 508

16.1.1 Cell search 508

16.1.2 Timing synchronization 509

16.2 Power control 509

16.2.1 Uplink power control 509

16.2.1.1 Narrowband physical uplink shared channel 509

16.2.1.1.1 UE behaviour 509

16.2.1.1.2 Power headroom 510

16.2.1.2 SR 510

16.2.1.2.1 UE behaviour 510

16.2.2 Downlink power allocation 511

16.3 Random access procedure 511

16.3.1 Physical non-synchronized random access procedure 511

16.3.2 Timing 512

16.3.3 Narrowband random access response grant 513

16.4 Narrowband physical downlink shared channel related procedures 515

16.4.1 UE procedure for receiving the narrowband physical downlink shared channel 515

16.4.1.1 Single-antenna port scheme 518

16.4.1.2 Transmit diversity scheme 518

16.4.1.3 Resource allocation 518

16.4.1.4 NPDSCH starting position 521

16.4.1.5 Modulation order and transport block size determination 522

16.4.1.5.1 Transport blocks not mapped for *SystemInformationBlockType1-NB* 522

16.4.1.5.2 Transport blocks mapped for *SystemInformationBlockType1-NB* 523

16.4.2 UE procedure for reporting ACK/NACK 523

16.5 Narrowband physical uplink shared channel related procedures 524

16.5.1 UE procedure for transmitting format 1 narrowband physical uplink shared channel 524

16.5.1.1 Resource allocation 526

16.5.1.2 Modulation order, redundancy version and transport block size determination 527

16.5.2 UE procedure for NPUSCH retransmission 529

16.5.3 UE procedure for transmitting SR 529

16.6 Narrowband physical downlink control channel related procedures 529

16.6.1 NPDCCH starting position 535

16.6.2 NPDCCH control information procedure 535

16.6.3 NPDCCH validation for semi-persistent scheduling 535

16.7 Assumptions independent of physical channel related to narrowband IoT 536

16.8 UE procedure for acquiring cell-specific reference signal sequence and raster offset 536

16.9 UE procedure for receiving narrowband wake up signal 536

17 Wake-up signal related procedures for BL/CE UE 537

Annex A (informative): Change history 538