3GPP TS 38.101-1 V15.20.0 (2022-12)

Technical Specification

3rd Generation Partnership Project;

Technical Specification Group Radio Access Network;

NR;

User Equipment (UE) radio transmission and reception;

Part 1: Range 1 Standalone

(Release 15)

** 

The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP.  
The present document has not been subject to any approval process by the 3GPPOrganizational Partners and shall not be implemented.  
This Specification is provided for future development work within 3GPPonly. The Organizational Partners accept no liability for any use of this Specification.  
Specifications and Reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organizational Partners' Publications Offices.

***3GPP***

Postal address

3GPP support office address

650 Route des Lucioles - Sophia Antipolis

Valbonne - FRANCE

Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16

Internet

http://www.3gpp.org

***Copyright Notification***

No part may be reproduced except as authorized by written permission.  
The copyright and the foregoing restriction extend to reproduction in all media.

© 2022, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

UMTS™ is a Trade Mark of ETSI registered for the benefit of its members

3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  
LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners

GSM® and the GSM logo are registered and owned by the GSM Association

Contents

Foreword 11

1 Scope 12

2 References 12

3 Definitions, symbols and abbreviations 12

3.1 Definitions 12

3.2 Symbols 13

3.3 Abbreviations 15

4 General 16

4.1 Relationship between minimum requirements and test requirements 16

4.2 Applicability of minimum requirements 16

4.3 Specification suffix information 16

5 Operating bands and channel arrangement 17

5.1 General 17

5.2 Operating bands 17

5.2A Operating bands for CA 18

5.2A.1 Intra-band CA 18

5.2A.2 Inter-band CA 19

5.2A.2.1 Inter-band CA (two bands) 19

5.2B Void 19

5.2C Operating band combination for SUL 19

5.3 UE channel bandwidth 20

5.3.1 General 20

5.3.2 Maximum transmission bandwidth configuration 21

5.3.3 Minimum guardband and transmission bandwidth configuration 21

5.3.4 RB alignment 22

5.3.5 UE channel bandwidth per operating band 22

5.3.6 Asymmetric channel bandwidths 24

5.3A UE channel bandwidth for CA 25

5.3A.1 General 25

5.3A.2 Maximum transmission bandwidth configuration for CA 25

5.3A.3 Minimum guardband and transmission bandwidth configuration for CA 25

5.3A.4 Void 27

5.3A.5 UE channel bandwidth per operating band for CA 27

5.4 Channel arrangement 27

5.4.1 Channel spacing 27

5.4.1.1 Channel spacing for adjacent NR carriers 27

5.4.2 Channel raster 28

5.4.2.1 NR-ARFCN and channel raster 28

5.4.2.2 Channel raster to resource element mapping 28

5.4.2.3 Channel raster entries for each operating band 29

5.4.3 Synchronization raster 30

5.4.3.1 Synchronization raster and numbering 30

5.4.3.2 Synchronization raster to synchronization block resource element mapping 31

5.4.3.3 Synchronization raster entries for each operating band 31

5.4.4 TX–RX frequency separation 32

5.4A Channel arrangement for CA 33

5.4A.1 Channel spacing for CA 33

5.4A.2 Channel raster for CA 33

5.4A.3 Synchronization raster for CA 34

5.4A.4 Tx-Rx frequency separation for CA 34

5.5 Void 34

5.5A Configurations for CA 34

5.5A.1 Configurations for intra-band contiguous CA 34

5.5A.2 Void 35

5.5A.3 Configurations for inter-band CA 35

5.5A.3.1 Configurations for inter-band CA (two bands) 35

5.5B Void 38

5.5C Configurations for SUL 38

6 Transmitter characteristics 39

6.1 General 39

6.2 Transmitter power 39

6.2.1 UE maximum output power 39

6.2.2 UE maximum output power reduction 40

6.2.3 UE additional maximum output power reduction 41

6.2.3.1 General 41

6.2.3.2 A-MPR for NS\_04 45

6.2.3.3 A-MPR for NS\_10 46

6.2.3.4 A-MPR for NS\_05 and NS\_05U 47

6.2.3.5 A-MPR for NS\_40 49

6.2.3.6 A-MPR for NS\_43 and NS\_43U 49

6.2.3.7 A-MPR for NS\_03 and NS\_03U 50

6.2.3.8 A-MPR for NS\_37 50

6.2.3.9 A-MPR for NS\_38 51

6.2.3.10 A-MPR for NS\_39 51

6.2.3.11 A-MPR for NS\_41 52

6.2.3.12 A-MPR for NS\_42 52

6.2.3.13 A-MPR for NS\_18 53

6.2.4 Configured transmitted power 54

6.2A Transmitter power for CA 56

6.2A.1 UE maximum output power for CA 56

6.2A.1.1 Void 56

6.2A.1.2 Void 56

6.2A.1.3 UE maximum output power for Inter-band CA 56

6.2A.2 UE maximum output power reduction for CA 56

6.2A.2.1 Void 56

6.2A.2.2 Void 56

6.2A.2.3 UE maximum output power reduction for Inter-band CA 56

6.2A.3 UE additional maximum output power reduction for CA 56

6.2A.3.1.1 Void 56

6.2A.3.1.2 Void 56

6.2A.3.1.3 UE additional maximum output power reduction for Inter-band CA 56

6.2A.4 Configured output power for CA 57

6.2A.4.1 Configured transmitted power level 57

6.2A.4.1.1 Void 57

6.2A.4.1.2 Void 57

6.2A.4.1.3 Configured transmitted power for Inter-band CA 57

6.2A.4.2 ΔTIB,c for CA 59

6.2A.4.2.1 Void 60

6.2A.4.2.2 Void 60

6.2A.4.2.3 ΔTIB,c for Inter-band CA (two bands) 60

6.2B Void 60

6.2C Transmitter power for SUL 60

6.2C.1 Configured transmitted power for SUL 60

6.2C.2 ΔTIB,c 60

6.2D Transmitter power for UL MIMO 61

6.2D.1 UE maximum output power for UL MIMO 61

6.2D.2 UE maximum output power reduction for UL MIMO 61

6.2D.3 UE additional maximum output power reduction for UL MIMO 62

6.2D.4 Configured transmitted power for UL MIMO 62

6.3 Output power dynamics 63

6.3.1 Minimum output power 63

6.3.2 Transmit OFF power 63

6.3.3 Transmit ON/OFF time mask 63

6.3.3.1 General 63

6.3.3.2 General ON/OFF time mask 64

6.3.3.3 Transmit power time mask for slot and short or long subslot boundaries 64

6.3.3.4 PRACH time mask 64

6.3.3.5 Void 65

6.3.3.6 SRS time mask 65

6.3.3.7 PUSCH-PUCCH and PUSCH-SRS time masks 67

6.3.3.8 Transmit power time mask for consecutive slot or long subslot transmission and short subslot transmission boundaries 68

6.3.3.9 Transmit power time mask for consecutive short subslot transmissions boundaries 68

6.3.4 Power control 69

6.3.4.1 General 69

6.3.4.2 Absolute power tolerance 69

6.3.4.3 Relative power tolerance 69

6.3.4.4 Aggregate power tolerance 70

6.3A Output power dynamics for CA 70

6.3A.1 Minimum output power for CA 70

6.3A.1.1 Void 70

6.3A.1.2 Void 70

6.3A.1.3 Minimum output power for inter-band CA 70

6.3A.2 Transmit OFF power for CA 71

6.3A.2.1 Void 71

6.3A.2.2 Void 71

6.3A.2.3 Transmit OFF power for inter-band CA 71

6.3A.3 Transmit ON/OFF time mask for CA 71

6.3A.3.1 Void 71

6.3A.3.2 Void 71

6.3A.3.3 Transmit ON/OFF time mask for inter-band CA 71

6.3A.4 Power control for CA 71

6.3A.4.1 Void 71

6.3A.4.2 Void 71

6.3A.4.3 Power control for inter-band CA 71

6.3D Output power dynamics for UL MIMO 71

6.3D.1 Minimum output power for UL MIMO 71

6.3D.2 Transmit OFF power for UL MIMO 71

6.3D.3 Transmit ON/OFF time mask for UL MIMO 72

6.3D.4 Power control for UL MIMO 72

6.4 Transmit signal quality 72

6.4.1 Frequency error 72

6.4.2 Transmit modulation quality 72

6.4.2.0 General 72

6.4.2.1 Error Vector Magnitude 72

6.4.2.2 Carrier leakage 73

6.4.2.3 In-band emissions 73

6.4.2.4 EVM equalizer spectrum flatness 74

6.4.2.4.1 Requirements for Pi/2 BPSK modulation 75

6.4A Transmit signal quality for CA 76

6.4A.1 Frequency error for CA 76

6.4A.1.1 Void 76

6.4A.1.2 Void 76

6.4A.1.3 Frequency error for inter-band CA 76

6.4A.2 Transmit modulation quality for CA 76

6.4A.2.1 Void 76

6.4A.2.2 Void 76

6.4A.2.3 Transmit modulation quality for inter-band CA 76

6.4D Transmit signal quality for UL MIMO 77

6.4D.0 General 77

6.4D.1 Frequency error for UL MIMO 77

6.4D.2 Transmit modulation quality for UL MIMO 77

6.4D.2.0 General 77

6.4D.2.1 Error Vector Magnitude 77

6.4D.2.2 Carrier leakage 77

6.4D.2.3 In-band emissions 78

6.4D.2.4 EVM equalizer spectrum flatness for UL MIMO 78

6.4D.3 Time alignment error for UL MIMO 78

6.4D.4 Requirements for coherent UL MIMO 78

6.5 Output RF spectrum emissions 78

6.5.1 Occupied bandwidth 78

6.5.2 Out of band emission 79

6.5.2.1 General 79

6.5.2.2 Spectrum emission mask 79

6.5.2.3 Additional spectrum emission mask 80

6.5.2.3.1 Requirements for network signalling value "NS\_35" 80

6.5.2.3.2 Requirements for network signalling value "NS\_04" 80

6.5.2.3.3 Requirements for network signalling values "NS\_03" and “NS\_03U” 81

6.5.2.3.4 Requirements for network signalling value "NS\_06" 82

6.5.2.3.5 Void 82

6.5.2.3.6 Void 82

6.5.2.3.7 Void 82

6.5.2.4 Adjacent channel leakage ratio 82

6.5.2.4.1 NR ACLR 83

6.5.2.4.2 UTRA ACLR 83

6.5.3 Spurious emissions 84

6.5.3.0 General 84

6.5.3.1 General spurious emissions 84

6.5.3.2 Spurious emissions for UE co-existence 84

6.5.3.3 Additional spurious emissions 89

6.5.3.3.1 Requirement for network signalling value "NS\_04" 89

6.5.3.3.2 Requirement for network signalling value "NS\_17" 90

6.5.3.3.3 Requirement for network singalling value "NS\_18" 90

6.5.3.3.4 Requirement for network signalling values "NS\_05" and “NS\_05U” 90

6.5.3.3.5 Requirement for network signalling values "NS\_43" and “NS\_43U” 90

6.5.3.3.6 Requirement for network signalling value "NS\_37" 91

6.5.3.3.7 Requirement for network signalling value "NS\_38" 91

6.5.3.3.8 Requirement for network signalling value "NS\_39" 91

6.5.3.3.9 Requirement for network signalling value "NS\_40" 91

6.5.3.3.10 Requirement for network signalling value "NS\_41" 92

6.5.3.3.11 Requirement for network signalling value "NS\_42" 92

6.5.3.3.12 Void 92

6.5.3.3.13 Void 92

6.5.3.3.14 Void 92

6.5.3.3.15 Void 92

6.5.3.3.16 Requirement for network signalling value "NS\_50" 92

6.5.4 Transmit intermodulation 93

6.5A Output RF spectrum emissions for CA 93

6.5A.0 General 93

6.5A.1 Occupied bandwidth for CA 93

6.5A.1.1 Void 93

6.5A.1.2 Void 93

6.5A.1.3 Occupied bandwidth for Inter-band CA 93

6.5A.2 Out of band emission for CA 94

6.5A.2.1 General 94

6.5A.2.2 Spectrum emission mask 94

6.5A.2.2.1 Void 94

6.5A.2.2.2 Void 94

6.5A.2.2.3 Spectrum emission mask for Inter-band CA 94

6.5A.2.3 Additional spectrum emission mask 94

6.5A.2.3.1 Void 94

6.5A.2.3.2 Void 94

6.5A.2.3.3 Additional spectrum emission mask for Inter-band CA 94

6.5A.2.4 Adjacent channel leakage ratio 94

6.5A.2.4.1 NR ACLR 94

6.5A.2.4.1.1 Void 94

6.5A.2.4.1.2 Void 94

6.5A.2.4.1.3 NR ACLR for Inter-band CA 94

6.5A.2.4.2 UTRA ACLR 94

6.5A.2.4.2.1 Void 94

6.5A.2.4.2.2 Void 94

6.5A.2.4.2.3 UTRA ACLR for Inter-band CA 94

6.5A.3 Spurious emission for CA 94

6.5A.3.1 General spurious emissions 94

6.5A.3.2 Spurious emissions for UE co-existence 95

6.5A.3.2.1 Void 95

6.5A.3.2.2 Void 95

6.5A.3.2.3 Spurious emissions for UE co-existence for Inter-band CA 95

6.5A.4 Transmit intermodulation for CA 96

6.5A.4.1 Void 96

6.5A.4.2 Void 96

6.5A.4.3 Transmit intermodulation for Inter-band CA 96

6.5D Output RF spectrum emissions for UL MIMO 96

6.5D.1 Occupied bandwidth for UL MIMO 96

6.5D.2 Out of band emission for UL MIMO 96

6.5D.3 Spurious emission for UL MIMO 96

6.5D.4 Transmit intermodulation for UL MIMO 96

7 Receiver characteristics 97

7.1 General 97

7.2 Diversity characteristics 97

7.3 Reference sensitivity 97

7.3.1 General 97

7.3.2 Reference sensitivity power level 97

7.3.3 ΔRIB,c 103

7.3A Reference sensitivity for CA 103

7.3A.1 General 103

7.3A.2 Reference sensitivity power level for CA 103

7.3A.2.1 Reference sensitivity power level for Intra-band contiguous CA 103

7.3A.2.2 Void 103

7.3A.2.3 Reference sensitivity power level for Inter-band CA 103

7.3A.2.4 Void 104

7.3A.3 ΔRIB,c for CA 105

7.3A.3.1 General 105

7.3A.3.2 ΔRIB,c for Inter-band CA 105

7.3A.3.2.1 ΔRIB,c for two bands 105

7.3A.3.2.2 Void 105

7.3A.4 Reference sensitivity exceptions due to UL harmonic interference for CA 105

7.3A.5 Reference sensitivity exceptions due to intermodulation interference due to 2UL CA 108

7.3A.6 Reference sensitivity exceptions due to cross band isolation for CA 108

7.3B Void 109

7.3C Reference sensitivity for SUL 109

7.3C.1 General 109

7.3C.2 Reference sensitivity power level for SUL 109

7.3C.3 ΔRIB,c for SUL 111

7.3C.3.1 General 111

7.3C.3.2 SUL band combination 111

7.3C.3.2.1 ΔRIB,c for two bands 111

7.3D Reference sensitivity for UL MIMO 111

7.4 Maximum input level 111

7.4A Maximum input level for CA 112

7.4A.1 Maximum input level for Intra-band contiguous CA 112

7.4A.2 Void 112

7.4A.3 Maximum input level for Inter-band CA 112

7.4D Maximum input level for UL MIMO 112

7.5 Adjacent channel selectivity 113

7.5A Adjacent channel selectivity for CA 117

7.5A.1 Adjacent channel selectivity for Intra-band contiguous CA 117

7.5A.2 Void 119

7.5A.3 Adjacent channel selectivity Inter-band CA 119

7.5D Adjacent channel selectivity for UL MIMO 119

7.6 Blocking characteristics 119

7.6.1 General 119

7.6.2 In-band blocking 119

7.6.3 Out-of-band blocking 121

7.6.4 Narrow band blocking 125

7.6A Blocking characteristics for CA 126

7.6A.1 General 126

7.6A.2 In-band blocking for CA 126

7.6A.2.1 In-band blocking for Intra-band contiguous CA 126

7.6A.2.2 Void 127

7.6A.2.3 In-band blocking for Inter-band CA 127

7.6A.3 Out-of-band blocking for CA 127

7.6A.3.1 Out-of-band blocking for Intra-band contiguous CA 127

7.6A.3.2 Void 128

7.6A.3.3 Out-of-band blocking for Inter-band CA 128

7.6A.4 Narrow band blocking for CA 129

7.6A.4.1 Narrow band blocking for Intra-band contiguous CA 129

7.6A.4.2 Void 130

7.6A.4.3 Narrow band blocking for Inter-band CA 130

7.6C Blocking characteristics for SUL 130

7.6C.1 General 130

7.6C.2 In-band blocking for SUL 130

7.6C.3 Out-of-band blocking for SUL 130

7.6C.4 Narrow band blocking for SUL 131

7.6D Blocking characteristics for UL MIMO 131

7.7 Spurious response 131

7.7A Spurious response for CA 133

7.7A.1 Spurious response for Intra-band contiguous CA 133

7.7A.2 Void 133

7.7A.3 Spurious response for Inter-band CA 133

7.7D Spurious response for UL MIMO 133

7.8 Intermodulation characteristics 133

7.8.1 General 133

7.8.2 Wide band Intermodulation 133

7.8A Intermodulation characteristics for CA 136

7.8A.1 General 136

7.8A.2 Wide band intermodulation for CA 136

7.8A.2.1 Wide band intermodulation for Intra-band contiguous CA 136

7.8A.2.2 Void 137

7.8A.2.3 Wide band intermodulation for Inter-band CA 137

7.8D Intermodulation characteristics for UL MIMO 137

7.9 Spurious emissions 137

7.9A Spurious emissions for CA 138

7.9A.1 Void 138

7.9A.2 Void 138

7.9A.3 Spurious emissions for Inter-band CA 138

Annex A (normative): Measurement channels 138

A.1 General 138

A.2 UL reference measurement channels 138

A.2.1 General 138

A.2.2 Reference measurement channels 139

A.2.2.1 DFT-s-OFDM Pi/2-BPSK 139

A.2.2.2 DFT-s-OFDM QPSK 140

A.2.2.3 DFT-s-OFDM 16QAM 141

A.2.2.4 DFT-s-OFDM 64QAM 142

A.2.2.5 DFT-s-OFDM 256QAM 143

A.2.2.6 CP-OFDM QPSK 144

A.2.2.7 CP-OFDM 16QAM 146

A.2.2.8 CP-OFDM 64QAM 149

A.2.2.9 CP-OFDM 256QAM 151

A.2.3 Reference measurement channels for TDD 153

A.2.3.1 DFT-s-OFDM Pi/2-BPSK 153

A.2.3.2 DFT-s-OFDM QPSK 153

A.2.3.3 DFT-s-OFDM 16QAM 153

A.2.3.4 DFT-s-OFDM 64QAM 153

A.2.3.5 DFT-s-OFDM 256QAM 153

A.2.3.6 CP-OFDM QPSK 154

A.2.3.7 CP-OFDM 16QAM 154

A.2.3.8 CP-OFDM 64QAM 154

A.2.3.9 CP-OFDM 256QAM 154

A.3 DL reference measurement channels 155

A.3.1 General 155

A.3.2 DL reference measurement channels for FDD 156

A.3.2.1 General 156

A.3.2.2 FRC for receiver requirements for QPSK 156

A.3.2.3 FRC for maximum input level for 64QAM 159

A.3.2.4 FRC for maximum input level for 256 QAM 162

A.3.3 DL reference measurement channels for TDD 165

A.3.3.1 General 165

A.3.3.2 FRC for receiver requirements for QPSK 166

A.3.3.3 FRC for maximum input level for 64QAM 169

A.3.3.4 FRC for maximum input level for 256 QAM 172

A.4 CSI reference measurement channels 175

A.5 OFDMA Channel Noise Generator (OCNG) 175

A.5.1 OCNG Patterns for FDD 175

A.5.1.1 OCNG FDD pattern 1: Generic OCNG FDD Pattern for all unused REs 175

A.5.2 OCNG Patterns for TDD 175

A.5.2.1 OCNG TDD pattern 1: Generic OCNG TDD Pattern for all unused REs 175

A.6 Void 175

Annex B (informative): Void 176

Annex C (informative): Downlink physical channels 177

C.1 General 177

C.2 Setup 177

C.3 Connection 177

C.3.1 Measurement of Receiver Characteristics 177

Annex D (normative): Characteristics of the interfering signal 178

D.1 General 178

D.2 Interference signals 178

Annex E (normative): Environmental conditions 179

E.1 General 179

E.2 Environmental 179

E.2.1 Temperature 179

E.2.2 Voltage 179

E.2.3 Vibration 180

Annex F (normative): Transmit modulation 181

F.0 General 181

F.1 Measurement Point 181

F.2 Basic Error Vector Magnitude measurement 181

F.3 Basic in-band emissions measurement 182

F.4 Modified signal under test 182

F.5 Window length 184

F.5.1 Timing offset 184

F.5.2 Window length 184

F.5.3 Window length for normal CP 184

F.5.4 Window length for Extended CP 186

F.5.5 Window length for PRACH 186

F.6 Averaged EVM 187

F.7 Spectrum Flatness 188

F.8 188

F.9 188

F.10 EVM for UL MIMO 189

F10.1 General 189

F10.2 MIMO Equalization 190

F10.3 Layer processing 190

Annex G (normative): 192

G.0 General 192

G.1 Measurement Point 192

G.2 Relative Phase Error Measurement 193

G.2.1 Symbols and subcarriers used 193

G.2.2 CFO (carrier frequency offset) correction 193

G.2.3 Steps of the measurement method 193

Annex H (normative): ModifiedMPR-Behavior 194

H.1 Indication of modified MPR behavior 194

Annex I (informative): Void 194

Annex J (informative): Void 194

Annex K (informative): Void 194

Annex L (informative): Change history 195