3GPP TS 36.101 V15.20.0 (2022-09)

Technical Specification

3rd Generation Partnership Project;

Technical Specification Group Radio Access Network;

Evolved Universal Terrestrial Radio Access (E-UTRA);

User Equipment (UE) radio transmission and reception

(Release 15)

** 

The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP.  
The present document has not been subject to any approval process by the 3GPPOrganizational Partners and shall not be implemented.   
This Specification is provided for future development work within 3GPPonly. The Organizational Partners accept no liability for any use of this Specification.  
Specifications and reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organizational Partners' Publications Offices.

***3GPP***

Postal address

3GPP support office address

650 Route des Lucioles - Sophia Antipolis

Valbonne - FRANCE

Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16

Internet

http://www.3gpp.org

***Copyright Notification***

No part may be reproduced except as authorized by written permission.  
The copyright and the foregoing restriction extend to reproduction in all media.

© 2022, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

UMTS™ is a Trade Mark of ETSI registered for the benefit of its members

3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  
LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners

GSM® and the GSM logo are registered and owned by the GSM Association

Contents

Foreword 32

1 Scope 33

2 References 33

3 Definitions, symbols and abbreviations 33

3.1 Definitions 33

3.2 Symbols 35

3.3 Abbreviations 38

4 General 39

4.1 Relationship between minimum requirements and test requirements 39

4.2 Applicability of minimum requirements 40

4.3 Void 40

4.3A Applicability of minimum requirements (CA, UL-MIMO, ProSe, Dual Connectivity, UE category 0, UE category M1, UE category M2, UE category 1bis, UE category NB1 and NB2, V2X Communication, MBMS UE) 40

4.4 RF requirements in later releases 42

5 Operating bands and channel arrangement 42

5.1 General 42

5.2 Void 42

5.3 Void 42

5.4 Void 42

5.5 Operating bands 42

5.5A Operating bands for CA 45

5.5B Operating bands for UL-MIMO 61

5.5C Operating bands for Dual Connectivity 61

5.5D Operating bands for ProSe 64

5.5E Operating bands for UE category 0, UE category M1 and M2 and UE category 1bis 64

5.5F Operating bands for category NB1 and NB2 65

5.5G Operating bands for V2X Communication 65

5.6 Channel bandwidth 66

5.6.1 Channel bandwidths per operating band 67

5.6A Channel bandwidth for CA 70

5.6A.1 Channel bandwidths per operating band for CA 72

5.6B Channel bandwidth for UL-MIMO 160

5.6B.1 Void 161

5.6C Channel bandwidth for Dual Connectivity 161

5.6C.1 Void 161

5.6D Channel bandwidth for ProSe 161

5.6D.1 Channel bandwidths per operating band for ProSe 161

5.6F Channel bandwidth for category NB1 and NB2 162

5.6G Channel bandwidth for V2X Communication 163

5.6G.1 Channel bandwidths per operating band for V2X Communication 163

5.7 Channel arrangement 165

5.7.1 Channel spacing 165

5.7.1A Channel spacing for CA 165

5.7.1F Channel spacing for category NB1 and NB2 166

5.7.2 Channel raster 166

5.7.2A Channel raster for CA 166

5.7.2F Channel raster for category NB1 and NB2 166

5.7.3 Carrier frequency and EARFCN 166

5.7.3F Carrier frequency and EARFCN for category NB1 and NB2 169

5.7.4 TX–RX frequency separation 169

5.7.4A TX–RX frequency separation for CA 170

5.7.4E TX–RX frequency separation for category M1 and M2 170

5.7.4F TX–RX frequency separation for category NB1 and NB2 170

6 Transmitter characteristics 171

6.1 General 171

6.2 Transmit power 171

6.2.1 Void 171

6.2.2 UE maximum output power 171

6.2.2A UE maximum output power for CA 174

6.2.2B UE maximum output power for UL-MIMO 179

6.2.2C Void 182

6.2.2D UE maximum output power for ProSe 182

6.2.2E UE maximum output power for Category M1 and M2 UE 182

6.2.2F UE maximum output power for category NB1 and NB2 183

6.2.2G UE maximum output power for V2X Communication 184

6.2.3 UE maximum output power for modulation / channel bandwidth 186

6.2.3A UE Maximum Output power for modulation / channel bandwidth for CA 187

6.2.3B UE maximum output power for modulation / channel bandwidth for UL-MIMO 192

6.2.3D UE maximum output power for modulation / channel bandwidth for ProSe 192

6.2.3E UE maximum output power for modulation / channel bandwidth for category M1 and M2 193

6.2.3F UE maximum output power for modulation / channel bandwidth for category NB1 and NB2 195

6.2.3G UE maximum output power for modulation / channel bandwidth for V2X Communication 195

6.2.3G.1 MPR for Power class 3 V2X UE 195

6.2.3G.2 MPR for Power class 2 V2X UE 197

6.2.4 UE maximum output power with additional requirements 197

6.2.4A UE maximum output power with additional requirements for CA 216

6.2.4A.1 A-MPR for CA\_NS\_01 for CA\_1C 218

6.2.4A.2 A-MPR for CA\_NS\_02 for CA\_1C 219

6.2.4A.3 A-MPR for CA\_NS\_03 for CA\_1C 219

6.2.4A.4 A-MPR for CA\_NS\_04 220

6.2.4A.5 A-MPR for CA\_NS\_05 for CA\_38C 222

6.2.4A.6 A-MPR for CA\_NS\_06 223

6.2.4A.7 A-MPR for CA\_NS\_07 224

6.2.4A.8 A-MPR for CA\_NS\_08 225

6.2.4A.9 Void 226

6.2.4B UE maximum output power with additional requirements for UL-MIMO 226

6.2.4D UE maximum output power with additional requirements for ProSe 227

6.2.4E UE maximum output power with additional requirements for category M1 and M2 UE 227

6.2.4F UE maximum output power with additional requirements for category NB1 and NB2 UE 236

6.2.4G UE maximum output power with additional requirements for V2X Communication 237

6.2.5 Configured transmitted power 239

6.2.5A Configured transmitted power for CA 267

6.2.5B Configured transmitted power for UL-MIMO 271

6.2.5C Configured transmitted power for Dual Connectivity 272

6.2.5D Configured transmitted power for ProSe 273

6.2.5F Configured transmitted Power for category NB1 and NB2 275

6.2.5G Configured transmitted power for V2X Communication 276

6.3 Output power dynamics 280

6.3.1 (Void) 280

6.3.2 Minimum output power 280

6.3.2.1 Minimum requirement 280

6.3.2A UE Minimum output power for CA 280

6.3.2A.1 Minimum requirement for CA 280

6.3.2B UE Minimum output power for UL-MIMO 280

6.3.2B.1 Minimum requirement 281

6.3.2C Void 281

6.3.2D UE Minimum output power for ProSe 281

6.3.2F UE Minimum output power for category NB1 and NB2 281

6.3.2G UE Minimum output power for V2X Communication 281

6.3.3 Transmit OFF power 282

6.3.3.1. Minimum requirement 282

6.3.3A UE Transmit OFF power for CA 282

6.3.3A.1 Minimum requirement for CA 282

6.3.3B UE Transmit OFF power for UL-MIMO 283

6.3.3B.1 Minimum requirement 283

6.3.3D Transmit OFF power for ProSe 283

6.3.3F Transmit OFF power for category NB1 and NB2 283

6.3.3G Transmit OFF power for V2X Communication 284

6.3.4 ON/OFF time mask 284

6.3.4.1 General ON/OFF time mask 284

6.3.4.2 PRACH and SRS time mask 285

6.3.4.2.1 PRACH time mask 285

6.3.4.2.2 SRS time mask 286

6.3.4.3 Slot / Sub frame boundary time mask for subframe TTI 287

6.3.4.4 PUCCH / PUSCH / SRS time mask for subframe TTI 289

6.3.4.5 Symbol / Subslot boundary time mask for subslot TTI 291

6.3.4.6 Subslot PUCCH / subslot PUSCH / SRS time mask for subslot TTI 293

6.3.4.7 Symbol / Slot boundary time mask for slot TTI 296

6.3.4.8 Slot PUCCH / slot PUSCH / SRS time mask for slot TTI 296

6.3.4.9 Consecutive subslot and slot TTI or consecutive subslot and subframe TTI time mask 297

6.3.4.10 Consecutive subframe and subslot TTI or consecutive slot and subslot TTI time mask 297

6.3.4.11 Consecutive TTI and slot TTI or consecutive slot TTI and TTI time mask 298

6.3.4A ON/OFF time mask for CA 298

6.3.4B ON/OFF time mask for UL-MIMO 298

6.3.4D ON/OFF time mask for ProSe 299

6.3.4D.1 General time mask for ProSe 299

6.3.4D.2 PSSS/SSSS time mask 299

6.3.4D.3 PSSS / SSSS / PSBCH time mask 300

6.3.4D.4 PSSCH / SRS time mask 301

6.3.4F ON/OFF time mask for category NB1 and NB2 301

6.3.4F.1 General ON/OFF time mask 301

6.3.4F.2 NPRACH time mask 302

6.3.4G ON/OFF time mask for V2X Communication 302

6.3.4G.1 PSSS / SSSS / PSBCH time mask 302

6.3.5 Power Control 303

6.3.5.1 Absolute power tolerance 303

6.3.5.1.1 Minimum requirements 303

6.3.5.2 Relative Power tolerance 304

6.3.5.2.1 Minimum requirements 304

6.3.5.3 Aggregate power control tolerance 305

6.3.5.3.1 Minimum requirement 305

6.3.5A Power control for CA 305

6.3.5A.1 Absolute power tolerance 305

6.3.5A.1.1 Minimum requirements 305

6.3.5A.2 Relative power tolerance 306

6.3.5A.2.1 Minimum requirements 306

6.3.5A.3 Aggregate power control tolerance 306

6.3.5A.3.1 Minimum requirements 306

6.3.5B Power control for UL-MIMO 307

6.3.5D Power Control for ProSe 307

6.3.5D.1 Absolute power tolerance 307

6.3.5E Power control for category M1 and M2 307

6.3.5E.1 Absolute power tolerance 307

6.3.5E.2 Relative Power tolerance 307

6.3.5E.3 Aggregate power control tolerance 308

6.3.5E.3.1 Minimum requirement 308

6.3.5F Power Control for category NB1 and NB2 308

6.3.5F.1 Absolute power tolerance 309

6.3.5F.2 Relative power tolerance 309

6.3.5F.3 Aggregate power control tolerance for category NB1 and NB2 310

6.3.5F.3.1 Minimum requirement 310

6.3.5G Power Control for V2X Communication 310

6.3.5G.1 Absolute power tolerance 310

6.4 Void 311

6.5 Transmit signal quality 311

6.5.1 Frequency error 311

6.5.1A Frequency error for CA 311

6.5.1B Frequency error for UL-MIMO 311

6.5.1D Frequency error for ProSe 311

6.5.1E Frequency error for UE category M1 and M2 311

6.5.1F Frequency error for UE category NB1 and NB2 312

6.5.1G Frequency error for V2X Communication 312

6.5.2 Transmit modulation quality 312

6.5.2.1 Error Vector Magnitude 313

6.5.2.1.1 Minimum requirement 313

6.5.2.2 Carrier leakage 313

6.5.2.2.1 Minimum requirements 314

6.5.2.3 In-band emissions 314

6.5.2.3.1 Minimum requirements 314

6.5.2.4 EVM equalizer spectrum flatness 315

6.5.2.4.1 Minimum requirements 315

6.5.2A Transmit modulation quality for CA 316

6.5.2A.1 Error Vector Magnitude 317

6.5.2A.2 Carrier leakage for CA 317

6.5.2A.2.1 Minimum requirements 317

6.5.2A.3 In-band emissions 317

6.5.2A.3.1 Minimum requirement for CA 317

6.5.2B Transmit modulation quality for UL-MIMO 320

6.5.2B.1 Error Vector Magnitude 320

6.5.2B.2 Carrier leakage 320

6.5.2B.3 In-band emissions 320

6.5.2B.4 EVM equalizer spectrum flatness for UL-MIMO 320

6.5.2D Transmit modulation quality for ProSe 320

6.5.2D.1 Error Vector Magnitude 320

6.5.2D.2 Carrier leakage 321

6.5.2D.3 In-band emissions 321

6.5.2D.4 EVM equalizer spectrum flatness for ProSe 321

6.5.2E Transmit modulation quality for category M1 and M2 321

6.5.2E.1 Error Vector Magnitude 321

The Error Vector Magnitude is defined in section 6.5.2.1. 321

6.5.2E.2 Carrier leakage 321

6.5.2E.2.1 Minimum requirements 321

6.5.2E.3 In-band emissions 321

6.5.2E.3.1 Minimum requirements 321

6.5.2F Transmit modulation quality for Category NB1 and NB2 323

6.5.2F.1 Error Vector Magnitude 323

6.5.2F.2 Carrier leakage 323

6.5.2F.3 In-band emissions 323

6.5.2G Transmit modulation quality for V2X Communication 324

6.5.2G.1 Error Vector Magnitude 324

6.5.2G.2 Carrier leakage 325

6.5.2G.3 In-band emissions 325

6.5.2G.4 EVM equalizer spectrum flatness 325

6.6 Output RF spectrum emissions 325

6.6.1 Occupied bandwidth 325

6.6.1.1 Additional minimum requirement for E-UTRA (network signalled value “NS\_29”) 326

6.6.1A Occupied bandwidth for CA 326

6.6.1B Occupied bandwidth for UL-MIMO 326

6.6.1F Occupied bandwidth for category NB1 and NB2 327

6.6.1G Occupied bandwidth for V2X Communication 327

6.6.2 Out of band emission 327

6.6.2.1 Spectrum emission mask 327

6.6.2.1.1 Minimum requirement 327

6.6.2.1A Spectrum emission mask for CA 328

6.6.2.2 Additional spectrum emission mask 329

6.6.2.2.1 Minimum requirement (network signalled value "NS\_03", “NS\_11”, "NS\_20", and “NS\_21”) 329

6.6.2.2.2 Minimum requirement (network signalled value "NS\_04") 330

6.6.2.2.3 Minimum requirement (network signalled value "NS\_06" or “NS\_07”) 330

6.6.2.2.4 Minimum requirement (network signalled value "NS\_33" or “NS\_34”) 331

6.6.2.2.5 Minimum requirement (network signalled value “NS\_27” and “NS\_43”) 331

6.6.2.2.6 Minimum requirement (network signalled value "NS\_28”) 332

6.6.2.2.7 Minimum requirement (network signalled value "NS\_35") 332

6.6.2.2A Additional Spectrum Emission Mask for CA 333

6.6.2.2A.1 Minimum requirement (network signalled value "CA\_NS\_04") 333

6.6.2.2A.2 Minimum requirement CA\_66B (network signalled value "CA\_NS\_09") 333

6.6.2.2A.3 Minimum requirement CA\_66C (network signalled value "CA\_NS\_09") 334

6.6.2.3 Adjacent Channel Leakage Ratio 334

6.6.2.3.1 Minimum requirement E-UTRA 335

6.6.2.3.1a Additional minimum requirement for E-UTRA (network signalled value “NS\_29”) 336

6.6.2.3.1A Void 336

6.6.2.3.1Aa Void 336

6.6.2.3.2 Minimum requirements UTRA 336

6.6.2.3.2A Minimum requirement UTRA for CA 337

6.6.2.3.3A Minimum requirements for CA E-UTRA 339

6.6.2.4 Void 340

6.6.2.4.1 Void 340

6.6.2A Void 340

6.6.2B Out of band emission for UL-MIMO 340

6.6.2C Void 340

6.6.2D Out of band emission for ProSe 341

6.6.2F Out of band emission for category NB1 and NB2 341

6.6.2F.1 Spectrum emission mask 341

6.6.2F.2 Additional Spectrum Emission Mask for Category NB1 and NB2 341

6.6.2F.2.1 Minimum requirement (network signalled value "NS\_02") 341

6.6.2F.2.2 Minimum requirement (network signalled value "NS\_03") 342

6.6.2F.3 Adjacent Channel Leakage Ratio for category NB1 and NB2 342

6.6.2G Out of band emission for V2X Communication 342

6.6.3 Spurious emissions 343

6.6.3.1 Minimum requirements 343

6.6.3.1A Minimum requirements for CA 344

6.6.3.2 Spurious emission band UE co-existence 345

6.6.3.2A Spurious emission band UE co-existence for CA 353

6.6.3.3 Additional spurious emissions 367

6.6.3.3.1 Minimum requirement (network signalled value "NS\_05") 367

6.6.3.3.2 Minimum requirement (network signalled value “NS\_07”) 368

6.6.3.3.3 Minimum requirement (network signalled value “NS\_08”) 368

6.6.3.3.4 Minimum requirement (network signalled value “NS\_09”) 368

6.6.3.3.5 Minimum requirement (network signalled value "NS\_12") 369

6.6.3.3.6 Minimum requirement (network signalled value “NS\_13”) 369

6.6.3.3.7 Minimum requirement (network signalled value “NS\_14”) 369

6.6.3.3.8 Minimum requirement (network signalled value “NS\_15”) 369

6.6.3.3.9 Minimum requirement (network signalled value “NS\_16”) 370

6.6.3.3.10 Minimum requirement (network signalled value “NS\_17”) 370

6.6.3.3.11 Minimum requirement (network signalled value “NS\_18”) 370

6.6.3.3.12 Minimum requirement (network signalled value “NS\_19”) 370

6.6.3.3.13 Minimum requirement (network signalled value “NS\_11”) 371

6.6.3.3.14 Minimum requirement (network signalled value “NS\_20”) 371

6.6.3.3.15 Minimum requirement (network signalled value “NS\_21”) 371

6.6.3.3.16 Minimum requirement (network signalled value "NS\_22") 372

6.6.3.3.17 Minimum requirement (network signalled value “NS\_23”) 372

6.6.3.3.18 Void 373

6.6.3.3.19 Minimum requirement (network signalled value "NS\_04") 373

6.6.3.3.20 Minimum requirement (network signalled value “NS\_24”) 373

6.6.3.3.21 Minimum requirement (network signalled value “NS\_25”) 374

6.6.3.3.22 Minimum requirement (network signalled value “NS\_26”) 374

6.6.3.3.23 Minimum requirement (network signalled value “NS\_27” and “NS\_43”) 374

6.6.3.3.24 Minimum requirement (network signalled value “NS\_28”) 374

6.6.3.3.25 Minimum requirement (network signalled value “NS\_29”) 375

6.6.3.3.26 Minimum requirement (network signalled value “NS\_30”) 375

6.6.3.3.27 Minimum requirement (network signalled value “NS\_31”) 376

6.6.3.3.28 Minimum requirement (network signalled value “NS\_36”) 377

6.6.3.3.29 Minimum requirement (network signalled value “NS\_38”) 377

6.6.3.3.30 Minimum requirement (network signalled value “NS\_39”) 377

6.6.3.3.31 Minimum requirement (network signalled value “NS\_40” and “NS\_41”) 378

6.6.3.3.32 Minimum requirement (network signalled value “NS\_42”) 378

6.6.3.3.33 Minimum requirement (network signalled value “NS\_44”) 378

6.6.3.3.34 Void 378

6.6.3.3.35 Minimum requirement (network signalled value “NS\_56”) 378

6.6.3.3A Additional spurious emissions for CA 379

6.6.3.3A.1 Minimum requirement for CA\_1C (network signalled value "CA\_NS\_01") 379

6.6.3.3A.2 Minimum requirement for CA\_1C (network signalled value "CA\_NS\_02") 379

6.6.3.3A.3 Minimum requirement for CA\_1C (network signalled value "CA\_NS\_03") 380

6.6.3.3A.4 Minimum requirement for CA\_38C (network signalled value "CA\_NS\_05") 380

6.6.3.3A.5 Minimum requirement for CA\_7C (network signalled value "CA\_NS\_06") 380

6.6.3.3A.6 Minimum requirement for CA\_39C and CA\_39C-41A (network signalled value "CA\_NS\_07") 381

6.6.3.3A.7 Minimum requirement for CA\_42C (network signalled value "CA\_NS\_08") 381

6.6.3.3A.8 Minimum requirement for CA\_41C (network signalled value "CA\_NS\_04") 381

6.6.3.3A.9 Void 382

6.6.3A Void 382

6.6.3B Spurious emission for UL-MIMO 382

6.6.3C Void 382

6.6.3D Spurious emission for ProSe 382

6.6.3F Spurious emission for category NB1 and NB2 382

6.6.3G Spurious emission for V2X Communication 382

6.6A Void 386

6.6B Void 386

6.7 Transmit intermodulation 386

6.7.1 Minimum requirement 386

6.7.1A Minimum requirement for CA 387

6.7.1B Minimum requirement for UL-MIMO 387

6.7.1F Minimum requirement for category NB1 and NB2 387

6.7.1G Minimum requirement for V2X Communication 388

6.8 Void 388

6.8A Void 388

6.8B Time alignment error for UL-MIMO 388

6.8B.1 Minimum Requirements 388

6.8C Void 389

6.8D Void 389

6.8E Void 389

6.8F Void 389

6.8G Time alignment error 389

7 Receiver characteristics 389

7.1 General 389

7.2 Diversity characteristics 390

7.3 Reference sensitivity power level 390

7.3.1 Minimum requirements (QPSK) 390

7.3.1A Minimum requirements (QPSK) for CA 423

7.3.1B Minimum requirements (QPSK) for UL-MIMO 506

7.3.1D Minimum requirements (QPSK) for ProSe 506

7.3.1E Minimum requirements (QPSK) for UE category 0, M1, M2 and 1bis 508

7.3.1F Minimum requirements for UE category NB1 and NB2 516

7.3.1F.1 Reference sensitivity for UE category NB1 and NB2 516

7.3.1F.2 Void 517

7.3.1G Minimum requirements (QPSK) for V2X 517

7.3.2 Void 519

7.4 Maximum input level 519

7.4.1 Minimum requirements 520

7.4.1A Minimum requirements for CA 520

7.4.1B Minimum requirements for UL-MIMO 521

7.4.1D Minimum requirements for ProSe 521

7.4.1F Minimum requirements for category NB1 and NB2 522

7.4.1G Minimum requirements for V2X 522

7.4A Void 523

7.4A.1 Void 523

7.5 Adjacent Channel Selectivity (ACS) 523

7.5.1 Minimum requirements 523

7.5.1A Minimum requirements for CA 524

7.5.1B Minimum requirements for UL-MIMO 528

7.5.1D Minimum requirements for ProSe 528

7.5.1F Minimum requirements for category NB1 and NB2 529

7.5.1G Minimum requirements for V2X 530

7.6 Blocking characteristics 532

7.6.1 In-band blocking 532

7.6.1.1 Minimum requirements 532

7.6.1.1A Minimum requirements for CA 534

7.6.1.1D Minimum requirements for ProSe 537

7.6.1.1F Minimum requirements for category NB1 and NB2 538

7.6.1.1G Minimum requirements for V2X 538

7.6.2 Out-of-band blocking 540

7.6.2.1 Minimum requirements 540

7.6.2.1A Minimum requirements for CA 542

7.6.2.1D Minimum requirements for ProSe 545

7.6.2.1F Minimum requirements for category NB1 and NB2 545

7.6.2.1G Minimum requirements for V2X 546

7.6.3 Narrow band blocking 547

7.6.3.1 Minimum requirements 547

7.6.3.1A Minimum requirements for CA 548

7.6.3.1D Minimum requirements for ProSe 549

7.6A Void 550

7.6B Blocking characteristics for UL-MIMO 550

7.7 Spurious response 550

7.7.1 Minimum requirements 550

7.7.1A Minimum requirements for CA 551

7.7.1B Minimum requirements for UL-MIMO 552

7.7.1D Minimum requirements for ProSe 552

7.7.1F Minimum requirements for UE category NB1 and NB2 553

7.7.1G Minimum requirements for V2X 553

7.8 Intermodulation characteristics 554

7.8.1 Wide band intermodulation 554

7.8.1.1 Minimum requirements 554

7.8.1A Minimum requirements for CA 555

7.8.1B Minimum requirements for UL-MIMO 558

7.8.1D Minimum requirements for ProSe 558

7.8.1F Minimum requirements for category NB1 and NB2 559

7.8.1G Minimum requirements 559

7.8.2 Void 560

7.9 Spurious emissions 560

7.9.1 Minimum requirements 561

7.9.1A Minimum requirements 561

7.10 Receiver image 562

7.10.1 Void 562

7.10.1A Minimum requirements for CA 562

7.10.1G Minimum requirements for V2X Communication 562

8 Performance requirement 563

8.1 General 563

8.1.1 Receiver antenna capability 563

8.1.1.1 Simultaneous unicast and MBMS operations 564

8.1.1.2 Dual-antenna receiver capability in idle mode 564

8.1.2 Applicability of requirements 564

8.1.2.1 Applicability of requirements for different channel bandwidths 564

8.1.2.2 Definition of CA capability 564

8.1.2.2A Definition of dual connectivity capability 569

8.1.2.3 Applicability and test rules for different CA configurations and bandwidth combination sets 570

8.1.2.3A Applicability and test rules for different dual connectivity configuration and bandwidth combination set 573

8.1.2.3B Applicability and test rules for different TDD-FDD CA configurations and bandwidth combination sets 574

8.1.2.3C Applicability and test rules for SDR tests for 4Rx capable UEs 576

8.1.2.3D Applicability and test rules for different CA with LAA SCell(s) configurations and bandwidth combination sets 576

8.1.2.3E Applicability and test rules for SDR tests for 8Rx capable UEs 577

8.1.2.4 Test coverage for different number of component carriers 578

8.1.2.5 Applicability of performance requirements for Type B receiver 579

8.1.2.6 Applicability of performance requirements for 4Rx capable UEs 579

8.1.2.6.1 Applicability rule and antenna connection for single carrier tests with 2Rx 579

8.1.2.6.2 Applicability rule and antenna connection for CA and DC tests with 2Rx 581

8.1.2.6.3 Applicability rule and antenna connection for single carrier tests with 4Rx 581

8.1.2.6.4 Applicability rule for 256QAM tests 582

8.1.2.6.5 Applicability rule and antenna connection for CA and DC tests with 4Rx 582

8.1.2.6.6 Applicability rule for Type C with 4Rx 586

8.1.2.6.7 Applicability rule for 1024QAM tests 586

8.1.2.7 Applicability of Enhanced Downlink Control Channel Performance Requirements 586

8.1.2.8 Applicability of performance requirements for CDM-multiplexed DM RS with interfering simultaneous transmission (FRC) with multiple CSI-RS configurations 588

8.1.2.8A Applicability of performance requirements for UE supporting coverage enhancement 588

8.1.2.9 Applicability of SDR requirements for CA and LAA 589

8.1.2.10 Applicability of performance requirements for Multi-user Superposed Transmission 590

8.1.2.11 Applicability CRS interference mitigation receivers performance requirements 590

8.1.2.12 Applicability of performance requirements for 8Rx capable UEs 591

8.1.2.12.1 Applicability rule and antenna connection for single carrier PDSCH tests 591

8.1.2.12.2 Applicability rule and antenna connection for control channel tests 597

8.1.2.12.3 Applicability rule and antenna connection for CA and DC tests 597

8.1.3 UE category and UE DL category 598

8.2 Demodulation of PDSCH (Cell-Specific Reference Symbols) 598

8.2.1 FDD (Fixed Reference Channel) 598

8.2.1.1 Single-antenna port performance 599

8.2.1.1.1 Minimum Requirement 599

8.2.1.1.2 Void 605

8.2.1.1.3 Void 605

8.2.1.1.4 Minimum Requirement 1 PRB allocation in presence of MBSFN 605

8.2.1.1.4A Minimum Requirement 1 PRB allocation in presence of FeMBMS Unicast-mixed Cell under CA 605

8.2.1.2 Transmit diversity performance 606

8.2.1.2.1 Minimum Requirement 2 Tx Antenna Port 606

8.2.1.2.2 Minimum Requirement 4 Tx Antenna Port 607

8.2.1.2.3 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS) 607

8.2.1.2.3A Minimum Requirement 2 Tx Antenna Ports (demodulation subframe overlaps with aggressor cell ABS and CRS assistance information are configured) 609

8.2.1.2.4 Enhanced Performance Requirement Type A - 2 Tx Antenna Ports with TM3 interference model 611

8.2.1.2.5 Enhanced Performance Requirement Type B - 2 Tx Antenna Ports with TM2 interference model 613

8.2.1.2.6 Enhanced Performance Requirement Type B - 2 Tx Antenna Ports with TM9 interference model 614

8.2.1.2.7 Minimum Requirement 2 Tx Antenna Port (Superposed transmission) 615

8.2.1.3 Open-loop spatial multiplexing performance 615

8.2.1.3.1 Minimum Requirement 2 Tx Antenna Port 615

8.2.1.3.1A Soft buffer management test 619

8.2.1.3.1B Enhanced Performance Requirement Type C –2Tx Antenna Ports 620

8.2.1.3.1C Enhanced Performance Requirement Type C - 2 Tx Antenna Ports with TM1 interference 621

8.2.1.3.2 Minimum Requirement 4 Tx Antenna Port 622

8.2.1.3.3 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS) 622

8.2.1.3.4 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS and CRS assistance information are configured) 626

8.2.1.3.5 Minimum Requirement 2 Tx Antenna Port (Superposed transmission) 628

8.2.1.3.6 Minimum Requirement 2 Tx Antenna Port (network-based CRS interference mitigation) 629

8.2.1.4 Closed-loop spatial multiplexing performance 630

8.2.1.4.1 Minimum Requirement Single-Layer Spatial Multiplexing 2 Tx Antenna Port 630

8.2.1.4.1A Minimum Requirement Single-Layer Spatial Multiplexing 4 Tx Antenna Port 631

8.2.1.4.1B Enhanced Performance Requirement Type A - Single-Layer Spatial Multiplexing 2 Tx Antenna Port with TM4 interference model 631

8.2.1.4.1C Minimum Requirement Single-Layer Spatial Multiplexing 2 Tx Antenna Ports (demodulation subframe overlaps with aggressor cell ABS and CRS assistance information are configured) 633

8.2.1.4.1D Enhanced Performance Requirement Type B - Single-layer Spatial Multiplexing 2 Tx Antenna Port with TM4 interference model 636

8.2.1.4.1E Minimum Requirement Single-Layer Spatial Multiplexing 2 Tx Antenna Ports with CRS assistance information 638

8.2.1.4.1F Minimum Requirement Single-Layer Spatial Multiplexing 4 Tx Antenna Ports with CRS assistance information 639

8.2.1.4.2 Minimum Requirement Multi-Layer Spatial Multiplexing 2 Tx Antenna Port 640

8.2.1.4.2A Enhanced Performance Requirement Type C – Multi-layer Spatial Multiplexing 2Tx Antenna Ports 641

8.2.1.4.3 Minimum Requirement Multi-Layer Spatial Multiplexing 4 Tx Antenna Port 641

8.2.1.4.3A Minimum Requirement Multi-Layer Spatial Multiplexing 4 Tx Antenna Port for dual connectivity 645

8.2.1.4.4 Minimum Requirement Multi-Layer Spatial Multiplexing 2 Tx Antenna Port (Superposed transmission) 647

8.2.1.5 MU-MIMO 648

8.2.1.6 [Control channel performance: D-BCH and PCH] 648

8.2.1.7 Carrier aggregation with power imbalance 648

8.2.1.7.1 Minimum Requirement 648

8.2.1.8 Intra-band non-contiguous carrier aggregation with timing offset 649

8.2.1.8.1 Minimum Requirement 649

8.2.1.9 HST-SFN performance 650

8.2.1.9.1 Minimum Requirement 650

8.2.1.10 Intra-band contiguous carrier aggregation with minimum channel spacing 651

8.2.1.10.1 Minimum Requirement 651

8.2.2 TDD (Fixed Reference Channel) 652

8.2.2.1 Single-antenna port performance 652

8.2.2.1.1 Minimum Requirement 652

8.2.2.1.2 Void 657

8.2.2.1.3 Void 657

8.2.2.1.4 Minimum Requirement 1 PRB allocation in presence of MBSFN 657

8.2.2.2 Transmit diversity performance 657

8.2.2.2.1 Minimum Requirement 2 Tx Antenna Port 657

8.2.2.2.2 Minimum Requirement 4 Tx Antenna Port 658

8.2.2.2.3 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS) 659

8.2.2.2.3A Minimum Requirement 2 Tx Antenna Ports (demodulation subframe overlaps with aggressor cell ABS and CRS assistance information are configured) 660

8.2.2.2.4 Enhanced Performance Requirement Type A – 2 Tx Antenna Ports with TM3 interference model 662

8.2.2.2.5 Minimum Requirement 2 Tx Antenna Port (when *EIMTA-MainConfigServCell-r12* is configured) 664

8.2.2.2.6 Enhanced Performance Requirement Type B - 2 Tx Antenna Ports with TM2 interference model 664

8.2.2.2.7 Enhanced Performance Requirement Type B - 2 Tx Antenna Ports with TM9 interference model 666

8.2.2.2.8 Minimum Requirement 2 Tx Antenna Port (Superposed transmission) 667

8.2.2.3 Open-loop spatial multiplexing performance 668

8.2.2.3.1 Minimum Requirement 2 Tx Antenna Port 668

8.2.2.3.1A Soft buffer management test 671

8.2.2.3.1B Enhanced Performance Requirement Type C - 2Tx Antenna Ports 671

8.2.2.3.1C Enhanced Performance Requirement Type C - 2 Tx Antenna Ports with TM1 interference 672

8.2.2.3.2 Minimum Requirement 4 Tx Antenna Port 673

8.2.2.3.3 Minimum Requirement 2Tx antenna port (demodulation subframe overlaps with aggressor cell ABS) 674

8.2.2.3.4 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS and CRS assistance information are configured) 678

8.2.2.3.5 Minimum Requirement 2 Tx Antenna Port (Superposed transmission) 680

8.2.2.3.6 Minimum Requirement 2 Tx Antenna Port (network-based CRS interference mitigation) 681

8.2.2.4 Closed-loop spatial multiplexing performance 682

8.2.2.4.1 Minimum Requirement Single-Layer Spatial Multiplexing 2 Tx Antenna Port 682

8.2.2.4.1A Minimum Requirement Single-Layer Spatial Multiplexing 4 Tx Antenna Port 683

8.2.2.4.1B Enhanced Performance Requirement Type A – Single-Layer Spatial Multiplexing 2 Tx Antenna Port with TM4 interference model 683

8.2.2.4.1C Minimum Requirement Single-Layer Spatial Multiplexing 2 Tx Antenna Ports (demodulation subframe overlaps with aggressor cell ABS and CRS assistance information are configured) 685

8.2.2.4.1D Enhanced Performance Requirement Type B - Single-layer Spatial Multiplexing 2 Tx Antenna Port with TM4 interference model 687

8.2.2.4.1E Minimum Requirement Single-Layer Spatial Multiplexing 2 Tx Antenna Ports with CRS assistance information 689

8.2.2.4.1F Minimum Requirement Single-Layer Spatial Multiplexing 4 Tx Antenna Ports with CRS assistance information 690

8.2.2.4.2 Minimum Requirement Multi-Layer Spatial Multiplexing 2 Tx Antenna Port 692

8.2.2.4.2A Enhanced Performance Requirement Type C Multi-Layer Spatial Multiplexing 2 Tx Antenna Port 692

8.2.2.4.3 Minimum Requirement Multi-Layer Spatial Multiplexing 4 Tx Antenna Port 693

8.2.2.4.3A Minimum Requirement Multi-Layer Spatial Multiplexing 4 Tx Antenna Port for dual connectivity 697

8.2.2.4.4 Void 698

8.2.2.4.5 Minimum Requirement Multi-Layer Spatial Multiplexing 2 Tx Antenna Port (Superposed transmission) 698

8.2.2.5 MU-MIMO 699

8.2.2.6 [Control channel performance: D-BCH and PCH] 699

8.2.2.7 Carrier aggregation with power imbalance 699

8.2.2.7.1 Minimum Requirement 699

8.2.2.8 Intra-band contiguous carrier aggregation with minimum channel spacing 700

8.2.2.8.1 Minimum Requirement 700

8.2.2.9 HST-SFN performance 701

8.2.2.9.1 Minimum Requirement 701

8.2.3 TDD FDD CA (Fixed Reference Channel) 702

8.2.3.1 Single-antenna port performance 703

8.2.3.1.1 Minimum Requirement for FDD PCell 703

8.2.3.1.2 Minimum Requirement for TDD PCell 707

8.2.3.2 Open-loop spatial multiplexing performance 2Tx Antenna port 711

8.2.3.2.1 Minimum Requirement for FDD PCell 711

8.2.3.2.1A Soft buffer management test for FDD PCell 715

8.2.3.2.2 Minimum Requirement for TDD PCell 716

8.2.3.2.2A Soft buffer management test for TDD PCell 720

8.2.3.3 Closed-loop spatial multiplexing performance 4Tx Antenna Port 721

8.2.3.3.1 Minimum Requirement for FDD PCell 721

8.2.3.3.2 Minimum Requirement for TDD PCell 725

8.2.3.4 Minimum Requirement for Closed-loop spatial multiplexing performance 4Tx Antenna Port for dual connectivity 729

8.2.4 LAA 731

8.2.4.1 Closed-loop spatial multiplexing performance 4Tx Antenna Port 731

8.2.4.1.1 FDD PCell (FDD single carrier) 731

8.2.4.1.2 TDD PCell (TDD single carrier) 735

8.3 Demodulation of PDSCH (User-Specific Reference Symbols) 738

8.3.1 FDD 738

8.3.1.1 Single-layer Spatial Multiplexing 739

8.3.1.1A Enhanced Performance Requirement Type A – Single-layer Spatial Multiplexing with TM9 interference model 741

8.3.1.1B Single-layer Spatial Multiplexing (demodulation subframe overlaps with aggressor cell ABS and CRS assistance information are configured) 744

8.3.1.1C Enhanced Performance Requirement Type B – Single-layer Spatial Multiplexing with TM9 interference model 747

8.3.1.1D Enhanced Performance Requirement Type B – Single-layer Spatial Multiplexing with CRS interference model 749

8.3.1.1E Enhanced Performance Requirement Type B – Single-layer Spatial Multiplexing with TM3 interference model 750

8.3.1.1F Enhanced Performance Requirement Type B – Single-layer Spatial Multiplexing with TM10 serving cell configuration and TM9 interference model 751

8.3.1.1G Single-layer Spatial Multiplexing (CRS assistance information is configured) 753

8.3.1.1H Single-layer Spatial Multiplexing (With Enhanced DMRS table configured) 755

8.3.1.1I Single-layer Spatial Multiplexing (with assistance information for simultaneous transmition interfering PDSCH) 756

8.3.1.2 Dual-Layer Spatial Multiplexing 758

8.3.1.2A Enhanced Performance Requirement Type C - Dual-Layer Spatial Multiplexing 759

8.3.1.3 Performance requirements for DCI format 2D and non Quasi Co-located Antenna Ports 760

8.3.1.3.1 Minimum requirement with Same Cell ID (with single NZP CSI-RS resource) 760

8.3.1.3.2 Minimum requirements with Same Cell ID (with multiple NZP CSI-RS resources) 762

8.3.1.3.3 Minimum requirement with Different Cell ID and Colliding CRS (with single NZP CSI-RS resource) 764

8.3.1.3.4 Minimum requirement with Different Cell ID and non-colliding CRS (with single NZP CSI-RS resource and CRS assistance information is configured) 766

8.3.1.3.5 Minimum requirements with different Cell ID and non-colliding CRS (with multiple NZP CSI-RS resources and CRS assistance information is configured) 768

8.3.1.3.6 Minimum requirements for QCL Type C and 2 Layers Spatial Multiplexing 771

8.3.1.4 Performance Requirements for semiOpenLoop transmission 773

8.3.2 TDD 775

8.3.2.1 Single-layer Spatial Multiplexing 775

8.3.2.1A Single-layer Spatial Multiplexing (with multiple CSI-RS configurations) 777

8.3.2.1B Enhanced Performance Requirement Type A – Single-layer Spatial Multiplexing with TM9 interference model 779

8.3.2.1C Single-layer Spatial Multiplexing (demodulation subframe overlaps with aggressor cell ABS and CRS assistance information are configured) 782

8.3.2.1D Enhanced Performance Requirement Type B – Single-layer Spatial Multiplexing with TM9 interference 785

8.3.2.1E Enhanced Performance Requirement Type B – Single-layer Spatial Multiplexing with CRS interference model 787

8.3.2.1F Enhanced Performance Requirement Type B – Single-layer Spatial Multiplexing with TM3 interference 789

8.3.2.1G Enhanced Performance Requirement Type B – Single-layer Spatial Multiplexing with TM10 serving cell configuration and TM9 interference model 790

8.3.2.1H Single-layer Spatial Multiplexing (CRS assistance information is configured) 792

8.3.2.1I Single-layer Spatial Multiplexing (With Enhanced DMRS table configured) 794

8.3.2.1J Single-layer Spatial Multiplexing (with assistance information for simultaneous transmition interfering PDSCH) 795

8.3.2.2 Dual-Layer Spatial Multiplexing 797

8.3.2.2A Enhanced Performance Requirement Type C - Dual-Layer Spatial Multiplexing 797

8.3.2.3 Dual-Layer Spatial Multiplexing (with multiple CSI-RS configurations) 798

8.3.2.4 Performance requirements for DCI format 2D and non Quasi Co-located Antenna Ports 799

8.3.2.4.1 Minimum requirement with Same Cell ID (with single NZP CSI-RS resource) 799

8.3.2.4.2 Minimum requirements with Same Cell ID (with multiple NZP CSI-RS resources) 801

8.3.2.4.3 Minimum requirement with Different Cell ID and Colliding CRS (with single NZP CSI-RS resource) 803

8.3.2.4.4 Minimum requirement with Different Cell ID and non-Colliding CRS (with single NZP CSI-RS resource and CRS assistance information is configured) 805

8.3.2.4.5 Minimum requirements with different Cell ID and non-colliding CRS (with multiple NZP CSI-RS resources and CRS assistance information is configured) 807

8.3.2.4.6 Minimum requirements for QCL Type C and 2 Layers Spatial Multiplexing 810

8.3.2.5 Performance Requirements for semiOpenLoop transmission 812

8.3.3 LAA 814

8.3.3.1 Dual-Layer Spatial Multiplexing with DM-RS 814

8.3.3.1.1 FDD PCell (FDD single carrier) 814

8.3.3.1.2 TDD Pcell (TDD single carrier) 819

8.4 Demodulation of PDCCH/PCFICH 823

8.4.1 FDD 823

8.4.1.1 Single-antenna port performance 824

8.4.1.2 Transmit diversity performance 824

8.4.1.2.1 Minimum Requirement 2 Tx Antenna Port 824

8.4.1.2.2 Minimum Requirement 4 Tx Antenna Port 824

8.4.1.2.3 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS) 825

8.4.1.2.4 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS and CRS assistance information are configured) 830

8.4.1.2.5 Enhanced Downlink Control Channel Performance Requirement Type A - 2 Tx Antenna Port under Asynchronous Network 835

8.4.1.2.6 Enhanced Downlink Control Channel Performance Requirement Type A - 2 Tx Antenna Port with Non-Colliding CRS Dominant Interferer 836

8.4.1.2.7 Enhanced Downlink Control Channel Performance Requirement Type B - 2 Tx Antenna Port with Colliding CRS Dominant Interferer 837

8.4.1.2.8 Enhanced Downlink Control Channel Performance Requirement Type B - 2 Tx Antenna Port with Non-Colliding CRS Dominant Interferer 838

8.4.1.2.9 Enhanced Downlink Control Channel Performance Requirement Type A - 4 Tx Antenna Port with Non-Colliding CRS Dominant Interferer 839

8.4.2 TDD 840

8.4.2.1 Single-antenna port performance 841

8.4.2.2 Transmit diversity performance 841

8.4.2.2.1 Minimum Requirement 2 Tx Antenna Port 841

8.4.2.2.2 Minimum Requirement 4 Tx Antenna Port 842

8.4.2.2.3 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS) 842

8.4.2.2.4 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS and CRS assistance information are configured) 846

8.4.2.2.5 Enhanced Downlink Control Channel Performance Requirement Type A - 2 Tx Antenna Port with Colliding CRS Dominant Interferer 850

8.4.2.2.6 Enhanced Downlink Control Channel Performance Requirement Type A - 2 Tx Antenna Port with Non-Colliding CRS Dominant Interferer 851

8.4.2.2.7 Enhanced Downlink Control Channel Performance Requirement Type B - 2 Tx Antenna Port with Colliding CRS Dominant Interferer 852

8.4.2.2.8 Enhanced Downlink Control Channel Performance Requirement Type B - 2 Tx Antenna Port with Non-Colliding CRS Dominant Interferer 853

8.4.2.2.9 Enhanced Downlink Control Channel Performance Requirement Type A - 4 Tx Antenna Port with Non-Colliding CRS Dominant Interferer 854

8.4.3 LAA 855

8.4.3.1 Transmit diversity performance 855

8.4.3.1.1 FDD Pcell (FDD single carrier) 855

8.4.3.1.2 TDD Pcell (TDD single carrier) 856

8.5 Demodulation of PHICH 857

8.5.1 FDD 858

8.5.1.1 Single-antenna port performance 858

8.5.1.2 Transmit diversity performance 858

8.5.1.2.1 Minimum Requirement 2 Tx Antenna Port 858

8.5.1.2.2 Minimum Requirement 4 Tx Antenna Port 859

8.5.1.2.3 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS) 859

8.5.1.2.4 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS and CRS assistance information are configured) 861

8.5.1.2.5 Enhanced Downlink Control Channel Performance Requirement Type A - 2 Tx Antenna Ports under Asynchronous Network 864

8.5.1.2.6 Enhanced Downlink Control Channel Performance Requirement Type A - 2 Tx Antenna Ports with Non-Colliding CRS Dominant Interferer 865

8.5.1.2.7 Enhanced Downlink Control Channel Performance Requirement Type B - 2 Tx Antenna Ports with Colliding CRS Dominant Interferer 866

8.5.1.2.8 Enhanced Downlink Control Channel Performance Requirement Type B - 2 Tx Antenna Ports with Non-Colliding CRS Dominant Interferer 867

8.5.2 TDD 868

8.5.2.1 Single-antenna port performance 869

8.5.2.2 Transmit diversity performance 869

8.5.2.2.1 Minimum Requirement 2 Tx Antenna Port 869

8.5.2.2.2 Minimum Requirement 4 Tx Antenna Port 870

8.5.2.2.3 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS) 870

8.5.2.2.4 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS and CRS assistance information are configured) 872

8.5.2.2.5 Enhanced Downlink Control Channel Performance Requirement Type A - 2 Tx Antenna Ports with Colliding CRS Dominant Interferer 874

8.5.2.2.6 Enhanced Downlink Control Channel Performance Requirement Type A - 2 Tx Antenna Ports with Non-Colliding CRS Dominant Interferer 875

8.5.2.2.7 Enhanced Downlink Control Channel Performance Requirement Type B - 2 Tx Antenna Ports with Colliding CRS Dominant Interferer 876

8.5.2.2.8 Enhanced Downlink Control Channel Performance Requirement Type B - 2 Tx Antenna Ports with Non-Colliding CRS Dominant Interferer 877

8.6 Demodulation of PBCH 878

8.6.1 FDD 878

8.6.1.1 Single-antenna port performance 878

8.6.1.2 Transmit diversity performance 879

8.6.1.2.1 Minimum Requirement 2 Tx Antenna Port 879

8.6.1.2.2 Minimum Requirement 4 Tx Antenna Port 879

8.6.1.2.3 Minimum Requirement 2 Tx Antenna Port under Time Domain Measurement Resource Restriction with CRS Assistance Information 879

8.6.2 TDD 881

8.6.2.1 Single-antenna port performance 881

8.6.2.2 Transmit diversity performance 881

8.6.2.2.1 Minimum Requirement 2 Tx Antenna Port 881

8.6.2.2.2 Minimum Requirement 4 Tx Antenna Port 881

8.6.2.2.3 Minimum Requirement 2 Tx Antenna Port under Time Domain Measurement Resource Restriction with CRS Assistance Information 882

8.7 Sustained downlink data rate provided by lower layers 883

8.7.1 FDD (single carrier and CA) 883

8.7.2 TDD (single carrier and CA) 900

8.7.3 FDD (EPDCCH scheduling) 904

8.7.4 TDD (EPDCCH scheduling) 906

8.7.5 TDD FDD CA 908

8.7.5.1 Minimum Requirement FDD PCell 909

8.7.5.2 Minimum Requirement TDD PCell 917

8.7.6 FDD (DC) 926

8.7.7 TDD (DC) 933

8.7.8 TDD FDD (DC) 936

8.7.9 FDD (4 Rx) 939

8.7.10 TDD (4 Rx) 941

8.7.11 TDD FDD CA (4 Rx) 943

8.7.11.1 Void 945

8.7.12 LAA 945

8.7.12.1 FDD CA in licensed bands 945

8.7.12.2 TDD CA in licensed bands 947

8.7.12.3 TDD-FDD CA in licensed bands 949

8.7.13 FDD DC (4 Rx) 952

8.7.14 TDD DC (4 Rx) 953

8.7.15 TDD FDD DC (4 Rx) 955

8.7.16 FDD (1024QAM and up to 4Rx supported) 957

8.7.17 TDD (1024QAM and up to 4 Rx supported) 960

8.7.18 TDD FDD CA (1024QAM and up to 4 Rx supported) 962

8.7.19 TDD (8 Rx) 964

8.8 Demodulation of EPDCCH 966

8.8.1 Distributed Transmission 966

8.8.1.1 FDD 966

8.8.1.1.1 Void 967

8.8.1.2 TDD 967

8.8.1.2.1 Void 968

8.8.2 Localized Transmission with TM9 968

8.8.2.1 FDD 968

8.8.2.1.1 Void 969

8.8.2.1.2 Void 970

8.8.2.2 TDD 970

8.8.2.2.1 Void 971

8.8.2.2.2 Void 971

8.8.3 Localized transmission with TM10 Type B quasi co-location type 971

8.8.3.1 FDD 971

8.8.3.2 TDD 974

8.8.4 Enhanced Downlink Control Channel Performance Requirements Type A - Localized Transmission with CRS Interference Model 977

8.8.4.1 FDD 977

8.8.4.2 TDD 978

8.8.5 Enhanced Downlink Control Channel Performance Requirements Type A - Distributed Transmission with TM9 Interference Model 980

8.8.5.1 TDD 980

8.8.6 Enhanced Downlink Control Channel Performance Requirements Type A - Distributed Transmission with TM3 Interference Model 981

8.8.6.1 FDD 981

8.9 Demodulation (single receiver antenna) 982

8.9.1 PDSCH 982

8.9.1.1 FDD and half-duplex FDD (Fixed Reference Channel) 982

8.9.1.1.1 Transmit diversity performance (Cell-Specific Reference Symbols) 982

8.9.1.1.2 Closed-loop spatial multiplexing performance (Cell-Specific Reference Symbols) 983

8.9.1.1.3 Closed-loop spatial multiplexing performance (User-Specific Reference Symbols) 985

8.9.1.2 TDD (Fixed Reference Channel) 988

8.9.1.2.1 Transmit diversity performance (Cell-Specific Reference Symbols) 988

8.9.1.2.2 Closed-loop spatial multiplexing performance (Cell-Specific Reference Symbols) 989

8.9.1.2.3 Closed-loop spatial multiplexing performance (User-Specific Reference Symbols) 992

8.9.2 PHICH 994

8.9.2.1 FDD and half-duplex FDD 994

8.9.2.1.1 Transmit diversity performance 994

8.9.2.2 TDD 994

8.9.2.2.1 Transmit diversity performance 994

8.9.3 PBCH 995

8.9.3.1 FDD and half-duplex FDD 995

8.9.3.1.1 Transmit diversity performance 995

8.9.3.2 TDD 995

8.9.3.2.1 Transmit diversity performance 995

8.9.4 PDCCH/PCFICH 995

8.9.4.1 FDD and half-duplex FDD 995

8.9.4.1.1 Enhanced Downlink Control Channel Performance Requirement Type A - 2 Tx Antenna Port with Non-Colliding CRS Dominant Interferer 995

8.9.4.1.2 Enhanced Downlink Control Channel Performance Requirement Type A - 4 Tx Antenna Port with Non-Colliding CRS Dominant Interferer 996

8.9.4.2 TDD 997

8.9.4.2.1 Enhanced Downlink Control Channel Performance Requirement Type A - 2 Tx Antenna Port with Non-Colliding CRS Dominant Interferer 997

8.9.4.2.2 Enhanced Downlink Control Channel Performance Requirement Type A - 4 Tx Antenna Port with Non-Colliding CRS Dominant Interferer 998

8.10 Demodulation (4 receiver antenna ports) 999

8.10.1 PDSCH 999

8.10.1.1 FDD (Fixed Reference Channel) 999

8.10.1.1.1 Transmit diversity performance with 2Tx Antenna Ports (Cell-Specific Reference Symbols) 1000

8.10.1.1.1A Transmit diversity performance wit Enhanced Performance Requirement Type A - 2 Tx Antenna Ports with TM3 interference model 1001

8.10.1.1.2 Open-loop spatial multiplexing performance with 2Tx Antenna Ports (Cell-Specific Reference Symbols) 1002

8.10.1.1.3 Closed-loop spatial multiplexing Enhanced Performance Requirements Type A - Single-Layer Spatial Multiplexing 2 Tx Antenna Port with TM4 interference model (Cell-Specific Reference Symbols) 1002

8.10.1.1.4 Closed-loop spatial multiplexing performance, Dual-Layer Spatial Multiplexing 4 Tx Antenna Port (Cell-Specific Reference Symbols) 1003

8.10.1.1.4A Enhanced Performance Requirement Type C - Dual-Layer Spatial Multiplexing with 2Tx Antenna Ports 1004

8.10.1.1.5 Enhanced Performance Requirement Type A – Single-layer Spatial Multiplexing with TM9 interference model (User-Specific Reference Symbols) 1005

8.10.1.1.5A Single-layer Spatial Multiplexing (User-Specific Reference Symbols) 1008

8.10.1.1.5B Single-layer Spatial Multiplexing (With Enhanced DMRS table configured) 1009

8.10.1.1.6 Dual-Layer Spatial Multiplexing (User-Specific Reference Symbols) 1010

8.10.1.1.6A Enhanced Performance Requirement Type C - Dual-Layer Spatial Multiplexing 1012

8.10.1.1.6B Dual-Layer Spatial Multiplexing with altCQI-Table-1024QAM configured (User-Specific Reference Symbols) 1013

8.10.1.1.7 Open-loop spatial multiplexing, 3 Layer Multiplexing with 4 Tx Antenna Ports (Cell-Specific Reference Symbols) 1014

8.10.1.1.7A Enhanced Performance Requirement Type C - Open-loop spatial multiplexing, 3 Layer Multiplexing with 4 Tx Antenna Ports (Cell-Specific Reference Symbols) 1014

8.10.1.1.8 Closed-loop spatial multiplexing performance, 4 Layers spatial multiplexing 4 Tx antennas (Cell-Specific Reference Symbols) 1015

8.10.1.1.9 4 Layer Spatial Multiplexing (User-Specific Reference Symbols) 1015

8.10.1.1.9A Enhanced Performance Requirement Type C - 4 Layer Spatial Multiplexing (User-Specific Reference Symbols) 1017

8.10.1.1.10 Closed loop spatial multiplexing performance - Single-Layer Spatial Multiplexing 2 Tx Antenna Port with CRS assistance information (Cell-Specific Reference Symbols) 1018

8.10.1.1.11 Closed loop spatial multiplexing performance - Single-Layer Spatial Multiplexing 4 Tx Antenna Port with CRS assistance information (Cell-Specific Reference Symbols) 1019

8.10.1.1.12 Closed loop spatial multiplexing performance - Single-Layer Spatial Multiplexing with CRS assistance information (User-Specific Reference Symbols) 1020

8.10.1.1.13 Performance requirements for DCI format 2D and non Quasi Co-located Antenna Ports 1021

8.10.1.2 TDD (Fixed Reference Channel) 1025

8.10.1.2.1 Transmit diversity performance with 2Tx Antenna Ports (Cell-Specific Reference Symbols) 1025

8.10.1.2.1A Transmit diversity performance with Enhanced Performance Requirement Type A – 2 Tx Antenna Ports with TM3 interference model 1026

8.10.1.2.2 Open-loop spatial multiplexing performance with 2Tx Antenna Ports (Cell-Specific Reference Symbols) 1028

8.10.1.2.3 Closed-loop spatial multiplexing Enhanced Performance Requirements Type A - Single-Layer Spatial Multiplexing 2 Tx Antenna Port with TM4 interference model (Cell-Specific Reference Symbols) 1028

8.10.1.2.4 Closed-loop spatial multiplexing performance, Dual-Layer Spatial Multiplexing 4 Tx Antenna Ports (Cell-Specific Reference Symbols) 1029

8.10.1.2.4A Enhanced Performance Requirement Type C - Dual-Layer Spatial Multiplexing with 2Tx Antenna Ports 1030

8.10.1.2.5 Enhanced Performance Requirement Type A – Single-layer Spatial Multiplexing with TM9 interference model (User-Specific Reference Symbols) 1031

8.10.1.2.5A Single-layer Spatial Multiplexing (with multiple CSI-RS configurations) 1034

8.10.1.2.5B Single-layer Spatial Multiplexing (With Enhanced DMRS table configured) 1035

8.10.1.2.6 Dual-Layer Spatial Multiplexing (User-Specific Reference Symbols) 1036

8.10.1.2.6A Enhanced Performance Requirement Type C - Dual-Layer Spatial Multiplexing 1038

8.10.1.2.6B Dual-Layer Spatial Multiplexing with altCQI-Table-1024QAM configured (User-Specific Reference Symbols) 1039

8.10.1.2.7 Open-loop spatial multiplexing, 3 Layer Multiplexing with 4 Tx Antenna Ports (Cell-Specific Reference Symbols) 1040

8.10.1.2.7A Enhanced Performance Requirement Type C - Open-loop spatial multiplexing, 3 Layer Multiplexing with 4 Tx Antenna Ports (Cell-Specific Reference Symbols) 1040

8.10.1.2.8 Closed-loop spatial multiplexing performance, 4 Layers spatial multiplexing 4 Tx antennas 1041

8.10.1.2.9 4 Layer Spatial Multiplexing (User-Specific Reference Symbols) 1042

8.10.1.2.9A Enhanced Performance Requirement Type C - 4 Layer Spatial Multiplexing (User-Specific Reference Symbols) 1043

8.10.1.2.10 Closed loop spatial multiplexing performance - Single-Layer Spatial Multiplexing 2 Tx Antenna Port with CRS assistance information (Cell-Specific Reference Symbols) 1044

8.10.1.2.11 Closed loop spatial multiplexing performance - Single-Layer Spatial Multiplexing 4 Tx Antenna Port with CRS assistance information (Cell-Specific Reference Symbols) 1046

8.10.1.2.12 Closed loop spatial multiplexing performance - Single-Layer Spatial Multiplexing with CRS assistance information (User-Specific Reference Symbols) 1047

8.10.1.2.13 Performance requirements for DCI format 2D and non Quasi Co-located Antenna Ports 1049

8.10.2 PDCCH/PCFICH 1053

8.10.2.1 FDD 1053

8.10.2.1.1 Single-antenna port performance 1053

8.10.2.1.2 Transmit diversity performance with 2 Tx Antenna Ports 1054

8.10.2.1.3 Transmit diversity performance with 4 Tx Antenna Ports 1054

8.10.2.1.4 Enhanced Downlink Control Channel Performance Requirement Type A - 4 Tx Antenna Port with Non-Colliding CRS Dominant Interferer 1054

8.10.2.2 TDD 1056

8.10.2.2.1 Single-antenna port performance 1056

8.10.2.2.2 Transmit diversity performance with 2 Tx Antenna Ports 1056

8.10.2.2.3 Transmit diversity performance with 4 Tx Antenna Ports 1057

8.10.2.2.4 Enhanced Downlink Control Channel Performance Requirement Type A - 4 Tx Antenna Port with Non-Colliding CRS Dominant Interferer 1057

8.10.3 PHICH 1058

8.10.3.1 FDD 1058

8.10.3.1.1 Single Tx Antenna Port performance 1058

8.10.3.1.2 Transmit diversity performance with 2 Tx Antenna Ports 1059

8.10.3.1.3 Transmit diversity performance with 4 Tx Antenna Ports 1059

8.10.3.2 TDD 1059

8.10.3.2.1 Single Tx Antenna Port performance 1060

8.10.3.2.2 Transmit diversity performance with 2 Tx Antenna Ports 1060

8.10.3.2.3 Transmit diversity performance with 4 Tx Antenna Ports 1061

8.10.4 ePDCCH 1061

8.10.4.1 Distributed Transmission with 4Rx 1061

8.10.4.1.1 FDD 1061

8.10.4.1.2 TDD 1062

8.10.4.2 Localized Transmission with TM9 and 4Rx 1063

8.10.4.2.1 FDD 1063

8.10.4.2.2 TDD 1064

8.11 Demodulation (UE supporting coverage enhancement) 1065

8.11.1 PDSCH 1066

8.11.1.1 FDD and half-duplex FDD (Fixed Reference Channel) 1066

8.11.1.1.1 Closed-loop spatial multiplexing performance (Cell-Specific Reference Symbols) 1066

8.11.1.1.2 Closed-loop spatial multiplexing performance (User-Specific Reference Symbols) 1070

8.11.1.1.3 Transmit diversity performance (Cell-Specific Reference Symbols) 1072

8.11.1.2 TDD (Fixed Reference Channel) 1077

8.11.1.2.1 Closed-loop spatial multiplexing performance (Cell-Specific Reference Symbols) 1077

8.11.1.2.2 Closed-loop spatial multiplexing performance (User-Specific Reference Symbols) 1082

8.11.1.2.3 Transmit diversity performance (Cell-Specific Reference Symbols) 1084

8.11.2 MPDCCH 1088

8.11.2.1 FDD and half-duplex FDD 1089

8.11.2.1.1 CE Mode A 1090

8.11.2.1.2 CE Mode B 1091

8.11.2.1.3 CE Mode A with TM9 interference model 1091

8.11.2.1.4 CE Mode A with CRS interference model 1093

8.11.2.2 TDD 1094

8.11.2.2.1 CE Mode A 1095

8.11.2.2.2 CE Mode B 1096

8.11.2.2.3 CE Mode A with TM9 interference model 1096

8.11.2.2.4 CE Mode A with CRS interference model 1097

8.11.3 PBCH 1098

8.11.3.1 FDD and half-duplex FDD 1099

8.11.3.1.1 Transmit diversity performance 1099

8.11.3.2 TDD 1100

8.11.3.2.1 Transmit diversity performance 1100

8.12 Demodulation of Narrowband IoT 1101

8.12.1 NPDSCH 1101

8.12.1.1 Half-duplex FDD 1101

8.12.1.1.1 Minimum Requirements for In-band 1101

8.12.1.1.2 Minimum Requirements for Standalone/Guard-band 1102

8.12.1.1.3 Minimum Requirements for Standalone for UE Category NB2 1103

8.12.1.2 TDD 1104

8.12.1.2.1 Minimum Requirements for In-band 1105

8.12.1.2.2 Minimum Requirements for Standalone/Guard-band 1106

8.12.1.2.3 Minimum Requirements for Standalone for UE Category NB2 1106

8.12.2 NPDCCH 1107

8.12.2.1 Half-duplex FDD 1107

8.12.2.1.1 Single-antenna performance 1108

8.12.2.1.2 Transmit diversity performance 1108

8.12.2.2 TDD 1109

8.12.2.2.1 Single-antenna performance 1110

8.12.2.2.2 Transmit diversity performance 1110

8.12.3 Demodulation of NPBCH 1111

8.12.3.1 HD-FDD 1111

8.12.3.1.1 Single-antenna port performance with single NPBCH TTI 1111

8.12.3.1.2 Transmit diversity performance 1111

8.12.3.2 TDD 1112

8.12.3.2.1 Single-antenna port performance with single NPBCH TTI 1112

8.12.3.2.2 Transmit diversity performance 1112

8.13 Demodulation of PDSCH CA and DC(4 receiver antenna ports) 1112

8.13.1 FDD (CA and DC) 1112

8.13.1.1 Closed-loop spatial multiplexing performance 1113

8.13.1.1.1 Minimum Requirement Multi-Layer Spatial Multiplexing 4 Tx Antenna Port 1113

8.13.1.1.2 Minimum Requirement Multi-Layer Spatial Multiplexing 4 Tx Antenna Port for dual connectivity 1116

8.13.1.1.3 Minimum Requirement Multi-Layer Spatial Multiplexing 4 Tx Antenna Port with 256QAM 1118

8.13.1.1.4 Minimum Requirement Four-Layer Spatial Multiplexing 4 Tx Antenna Port 1120

8.13.1.2 Dual-Layer Spatial Multiplexing (User-Specific Reference Symbols) 1121

8.13.1.2.1 Minimum Requirement Dual-Layer Spatial Multiplexing 2 Tx Antenna Port 1121

8.13.1.3 Enhanced Performance Requirements Type A Closed-loop spatial multiplexing 1124

8.13.1.3.1 Minimum Requirement Single-Layer Spatial Multiplexing 2 Tx Antenna Port with TM4 interference model (Cell-Specific Reference Symbols) 1124

8.13.1.4 Enhanced Performance Requirement Type A - Single-layer Spatial Multiplexing (User-Specific Reference Symbols) 1126

8.13.1.4.1 Minimum Requirement Enhanced Performance Requirement Type A – Single-layer Spatial Multiplexing with TM9 interference model (User-Specific Reference Symbols) 1126

8.13.2 TDD (CA and DC) 1129

8.13.2.1 Closed-loop spatial multiplexing performance 1130

8.13.2.1.1 Minimum Requirement Multi-Layer Spatial Multiplexing 4 Tx Antenna Port 1130

8.13.2.1.2 Minimum Requirement Multi-Layer Spatial Multiplexing 4 Tx Antenna Port for dual connectivity 1132

8.13.2.1.3 Minimum Requirement Multi-Layer Spatial Multiplexing 4 Tx Antenna Port with 256QAM 1133

8.13.2.1.4 Minimum Requirement Four-Layer Spatial Multiplexing 4 Tx Antenna Port 1134

8.13.2.2 Dual-Layer Spatial Multiplexing (User-Specific Reference Symbols) 1136

8.13.2.2.1 Minimum Requirement Dual-Layer Spatial Multiplexing 2 Tx Antenna Port 1136

8.13.2.4 Enhanced Performance Requirement Type A - Single-layer Spatial Multiplexing (User-Specific Reference Symbols) 1140

8.13.2.4.1 Minimum Requirement Enhanced Performance Requirement Type A – Single-layer Spatial Multiplexing with TM9 interference model (User-Specific Reference Symbols) 1140

8.13.3 TDD-FDD (CA and DC) 1142

8.13.3.1 Closed-loop spatial multiplexing performance 4Tx Antenna Port 1143

8.13.3.1.1 Minimum Requirement for FDD PCell 1143

8.13.3.1.2 Minimum Requirement for TDD PCell 1146

8.13.3.2 Dual-Layer Spatial Multiplexing (User-Specific Reference Symbols) 1150

8.13.3.2.1 Minimum Requirement Dual-Layer Spatial Multiplexing 2 Tx Antenna Port for FDD PCell 1150

8.13.3.2.2 Minimum Requirement Dual-Layer Spatial Multiplexing 2 Tx Antenna Port for TDD PCell 1153

8.13.3.3 Enhanced Performance Requirements Type A Closed-loop spatial multiplexing 1156

8.13.3.3.1 Minimum Requirement Single-Layer Spatial Multiplexing 2 Tx Antenna Port with TM4 interference model (Cell-Specific Reference Symbols) for FDD PCell 1156

8.13.3.3.2 Minimum Requirement Single-Layer Spatial Multiplexing 2 Tx Antenna Port with TM4 interference model (Cell-Specific Reference Symbols) for TDD PCell 1158

8.13.3.4 Enhanced Performance Requirement Type A - Single-layer Spatial Multiplexing (User-Specific Reference Symbols) 1160

8.13.3.4.1 Minimum Requirement Enhanced Performance Requirement Type A – Single-layer Spatial Multiplexing with TM9 interference model (User-Specific Reference Symbols) for FDD PCell 1160

8.13.3.4.2 Minimum Requirement Enhanced Performance Requirement Type A – Single-layer Spatial Multiplexing with TM9 interference model (User-Specific Reference Symbols) for TDD PCell 1163

8.13.3.5 Closed-loop spatial multiplexing performance 4Tx Antenna Port for DC 1166

8.13.3.5.1 Minimum Requirement for FDD PCell 1166

8.13.3.5.2 Minimum Requirement for TDD PCell 1168

8.13.3.6 Closed-loop spatial multiplexing performance 4Tx Antenna Port with 256QAM 1170

8.13.3.6.1 Minimum Requirement for FDD PCell 1170

8.13.3.6.2 Minimum Requirement for TDD PCell 1172

8.13.3.7 Closed-loop spatial multiplexing performance 4Tx Antenna Port with Four layers 1173

8.13.3.7.1 Minimum Requirement for FDD PCell 1173

8.13.3.7.2 Minimum Requirement for TDD PCell 1175

8.14 Demodulation (UE supporting Short TTI) 1177

8.14.1 Slot-PDSCH and Subslot-PDSCH 1177

8.14.1.1 FDD (Fixed Reference Channel) 1177

8.14.1.1.1 Open-loop spatial multiplexing performance 1177

8.14.1.1.2 Closed-loop spatial multiplexing performance (User-Specific Reference Signals) 1178

8.14.1.2 TDD (Fixed Reference Channel) 1180

8.14.1.2.1 Open-loop spatial multiplexing performance 1180

8.14.1.2.2 Closed-loop spatial multiplexing performance (User-Specific Reference Signals) 1181

8.14.2 SPDCCH 1182

8.14.2.1 FDD 1182

8.14.2.1.1 Mimimum requirement 1183

8.14.2.2 TDD 1183

8.14.2.2.1 Mimimum requirement 1184

8.15 Demodulation (8 receiver antenna ports) 1185

8.15.1 PDSCH 1185

8.15.1.1 Void 1185

8.15.1.2 TDD (Fixed Reference Channel) 1185

8.15.1.2.1 Transmit diversity performance with 2Tx Antenna Ports (Cell-Specific Reference Symbols) 1185

8.15.1.2.2 Open-loop spatial multiplexing performance with 2Tx Antenna Ports (Cell-Specific Reference Symbols) 1186

8.15.1.2.3 8 Layer Spatial Multiplexing (User-Specific Reference Symbols) 1186

8.15.2 CA 1188

8.15.2.1 Void 1188

8.15.2.2 TDD 1188

8.15.2.2.1 Eight Layer Spatial Multiplexing (User-Specific Reference Symbols) 1188

9 Reporting of Channel State Information 1190

9.1 General 1190

9.1.1 Applicability of requirements 1190

9.1.1.1 Applicability of requirements for different channel bandwidths 1190

9.1.1.2 Applicability and test rules for different CA configurations and bandwidth combination sets 1190

9.1.1.2A Applicability and test rules for different TDD-FDD CA configurations and bandwidth combination sets 1191

9.1.1.3 Test coverage for different number of componenet carriers 1192

9.1.1.4 Applicability of performance requirements for 4Rx capable UEs 1192

9.1.1.4.1 Applicability rule and antenna connection for single carrier tests with 2Rx 1192

9.1.1.4.2 Applicability rule and antenna connection for CA tests with 2Rx 1194

9.1.1.4.3 Applicability rule and antenna connection for single carrier tests with 4Rx 1195

9.1.1.5 Applicability of requirements for UEs supporting coverage enhancement 1195

9.2 CQI reporting definition under AWGN conditions 1195

9.2.1 Minimum requirement PUCCH 1-0 (Cell-Specific Reference Symbols) 1195

9.2.1.1 FDD 1195

9.2.1.2 TDD 1196

9.2.1.3 FDD (CSI measurements in case two CSI subframe sets are configured) 1197

9.2.1.4 TDD (CSI measurements in case two CSI subframe sets are configured) 1200

9.2.1.5 FDD (CSI measurements in case two CSI subframe sets are configured and with CRS assistance information) 1203

9.2.1.6 TDD (CSI measurements in case two CSI subframe sets are configured and with CRS assistance information) 1206

9.2.1.7 FDD (Modulation and TBS index Table 2 and 4-bit CQI Table 2 are used) 1209

9.2.1.8 TDD (Modulation and TBS index Table 2 and 4-bit CQI Table 2 are used) 1210

9.2.1.9 FDD (Modulation and TBS index Table 3 and 4-bit CQI Table 4 are used) 1210

9.2.1.10 TDD (Modulation and TBS index Table 3 and 4-bit CQI Table 4 are used) 1211

9.2.2 Minimum requirement PUCCH 1-1 (Cell-Specific Reference Symbols) 1212

9.2.2.1 FDD 1212

9.2.2.2 TDD 1213

9.2.3 Minimum requirement PUCCH 1-1 (CSI Reference Symbols) 1214

9.2.3.1 FDD 1214

9.2.3.1A FDD (With *channelMeasRestriction* configured) 1215

9.2.3.2 TDD 1216

9.2.3.2A TDD (With *channelMeasRestriction* configured) 1217

9.2.4 Minimum requirement PUCCH 1-1 (With Single CSI Process) 1218

9.2.4.1 FDD 1219

9.2.4.1A FDD (With *interferenceMeasRestriction* configured) 1221

9.2.4.2 TDD 1224

9.2.4.2A TDD (With *interferenceMeasRestriction* configured) 1227

9.2.5 Minimum requirement PUCCH 1-1 (when *csi-SubframeSet –r12* and *EIMTA-MainConfigServCell-r12* are configured) 1230

9.2.6 Minimum requirement PUSCH 3-0 (Cell-Specific Reference Symbols) 1233

9.2.6.1 Frame structure type 3 with FDD Pcell 1233

9.2.6.2 Frame structure type 3 with TDD Pcell 1235

9.2.7 Minimum requirement PUSCH 3-1 (CSI Reference Symbol) 1237

9.2.7.1 Frame structure type 3 wth FDD Pcell 1237

9.2.7.2 Frame structure type 3 wth TDD Pcell 1239

9.3 CQI reporting under fading conditions 1243

9.3.1 Frequency-selective scheduling mode 1243

9.3.1.1 Minimum requirement PUSCH 3-0 (Cell-Specific Reference Symbols) 1243

9.3.1.1.1 FDD 1243

9.3.1.1.2 TDD 1244

9.3.1.1.3 FDD (CSI measurements in case two CSI subframe sets are configured and with CRS assistance information) 1245

9.3.1.1.4 TDD (CSI measurements in case two CSI subframe sets are configured and with CRS assistance information) 1249

9.3.1.1.5 TDD (when *csi-SubframeSet –r12* is configured) 1252

9.3.1.2 Minimum requirement PUSCH 3-1 (CSI Reference Symbol) 1254

9.3.1.2.1 FDD 1254

9.3.1.2.2 TDD 1255

9.3.1.2.3 FDD (Modulation and TBS index Table 2 and 4-bit CQI Table 2 are used) 1257

9.3.1.2.4 TDD (Modulation and TBS index Table 2 and 4-bit CQI Table 2 are used) 1258

9.3.1.2.5 Void 1259

9.3.1.2.6 TDD (when *csi-SubframeSet –r12* is configured with one CSI process) 1259

9.3.2 Frequency non-selective scheduling mode 1263

9.3.2.1 Minimum requirement PUCCH 1-0 (Cell-Specific Reference Symbol) 1263

9.3.2.1.1 FDD 1263

9.3.2.1.2 TDD 1265

9.3.2.2 Minimum requirement PUCCH 1-1 (CSI Reference Symbol) 1266

9.3.2.2.1 FDD 1266

9.3.2.2.2 TDD 1268

9.3.3 Frequency-selective interference 1270

9.3.3.1 Minimum requirement PUSCH 3-0 (Cell-Specific Reference Symbol) 1270

9.3.3.1.1 FDD 1270

9.3.3.1.2 TDD 1271

9.3.3.2 Void 1272

9.3.3.2.1 Void 1272

9.3.3.2.2 Void 1272

9.3.4 UE-selected subband CQI 1272

9.3.4.1 Minimum requirement PUSCH 2-0 (Cell-Specific Reference Symbols) 1272

9.3.4.1.1 FDD 1272

9.3.4.1.2 TDD 1273

9.3.4.2 Minimum requirement PUCCH 2-0 (Cell-Specific Reference Symbols) 1274

9.3.4.2.1 FDD 1274

9.3.4.2.2 TDD 1276

9.3.5 Additional requirements for enhanced receiver Type A 1278

9.3.5.1 Minimum requirement PUCCH 1-0 (Cell-Specific Reference Symbol) 1278

9.3.5.1.1 FDD 1278

9.3.5.1.2 TDD 1279

9.3.5.2 Minimum requirement PUCCH 1-1 (CSI Reference Symbol) 1281

9.3.5.2.1 FDD 1281

9.3.5.2.2 TDD 1284

9.3.6 Minimum requirement (With multiple CSI processes) 1287

9.3.6.1 FDD 1287

9.3.6.2 TDD 1292

9.3.7 Minimum requirement PUSCH 3-2 1296

9.3.7.1 FDD 1296

9.3.7.2 TDD 1297

9.3.8 Additional requirements for enhanced receiver Type B 1299

9.3.8.1 Minimum requirement PUCCH 1-1 (Cell-Specific Reference Symbols) 1299

9.3.8.1.1 FDD 1299

9.3.8.1.2 TDD 1300

9.3.8.2 Minimum requirement PUCCH 1-1 (CSI Reference Symbols) 1302

9.3.8.2.1 FDD 1302

9.3.8.2.2 TDD 1304

9.3.8.3 Minimum requirement with CSI process 1307

9.3.8.3.1 FDD 1307

9.3.8.3.2 TDD 1310

9.4 Reporting of Precoding Matrix Indicator (PMI) 1313

9.4.1 Single PMI 1314

9.4.1.1 Minimum requirement PUSCH 3-1 (Cell-Specific Reference Symbols) 1314

9.4.1.1.1 FDD 1314

9.4.1.1.2 TDD 1315

9.4.1.2 Minimum requirement PUCCH 2-1 (Cell-Specific Reference Symbols) 1316

9.4.1.2.1 FDD 1316

9.4.1.2.2 TDD 1318

9.4.1.3 Minimum requirement PUSCH 3-1 (CSI Reference Symbol) 1319

9.4.1.3.1 FDD 1319

9.4.1.3.2 TDD 1322

9.4.1.3.3 FDD (with Class A 12Tx codebook) 1325

9.4.1.3.4 TDD (with Class A 12Tx codebook) 1327

9.4.1.3.5 FDD (with Class A 24Tx codebook) 1330

9.4.1.3.6 TDD (with Class A 24Tx codebook) 1332

9.4.1.4 Minimum requirement PUCCH 1-1 (CSI Reference Symbol) 1335

9.4.1.4.1 FDD (with 4Tx enhanced codebook) 1335

9.4.1.4.2 TDD (with 4Tx enhanced codebook) 1337

9.4.1.4.3 FDD (with Class B alternative codebook for one CSI-RS resource configured) 1340

9.4.1.4.4 TDD (with Class B alternative codebook for one CSI-RS resource configured) 1342

9.4.1a Void 1345

9.4.1a.1 Void 1345

9.4.1a.1.1 Void 1345

9.4.1a.1.2 Void 1345

9.4.2 Multiple PMI 1345

9.4.2.1 Minimum requirement PUSCH 1-2 (Cell-Specific Reference Symbols) 1345

9.4.2.1.1 FDD 1345

9.4.2.1.2 TDD 1346

9.4.2.2 Minimum requirement PUSCH 2-2 (Cell-Specific Reference Symbols) 1347

9.4.2.2.1 FDD 1347

9.4.2.2.2 TDD 1348

9.4.2.3 Minimum requirement PUSCH 1-2 (CSI Reference Symbol) 1349

9.4.2.3.1 FDD 1349

9.4.2.3.2 TDD 1351

9.4.2.3.3 FDD (with 4Tx enhanced codebook) 1354

9.4.2.3.4 TDD (with 4Tx enhanced codebook) 1356

9.4.2.3.5 FDD (with Class A 16Tx codebook) 1358

9.4.2.3.6 TDD (with Class A 16Tx codebook) 1361

9.4.2.3.7 FDD (with Class A 32Tx codebook) 1364

9.4.2.3.8 TDD (with Class A 32Tx codebook) 1367

9.4.2.3.9 FDD (with Class A 16Tx advanced codebook) 1370

9.4.2.3.10 TDD (with Class A 16Tx advanced codebook) 1373

9.4.3 Void 1376

9.5 Reporting of Rank Indicator (RI) 1376

9.5.1 Minimum requirement (Cell-Specific Reference Symbols) 1376

9.5.1.1 FDD 1376

9.5.1.2 TDD 1377

9.5.2 Minimum requirement (CSI Reference Symbols) 1378

9.5.2.1 FDD 1378

9.5.2.2 TDD 1380

9.5.3 Minimum requirement (CSI measurements in case two CSI subframe sets are configured) 1382

9.5.3.1 FDD 1382

9.5.3.2 TDD 1385

9.5.4 Minimum requirement (CSI measurements in case two CSI subframe sets are configured and CRS assistance information are configured) 1388

9.5.4.1 FDD 1388

9.5.4.2 TDD 1391

9.5.5 Minimum requirement (with CSI process) 1394

9.5.5.1 FDD 1395

9.5.5.2 TDD 1398

9.6 Additional requirements for carrier aggregation 1401

9.6.1 Periodic reporting on multiple cells (Cell-Specific Reference Symbols) 1401

9.6.1.1 FDD 1401

9.6.1.2 TDD 1407

9.6.1.3 TDD-FDD CA with FDD PCell 1413

9.6.1.4 TDD-FDD CA with TDD PCell 1418

9.7 CSI reporting (Single receiver antenna) 1424

9.7.1 CQI reporting definition under AWGN conditions 1425

9.7.1.1 FDD and half-duplex FDD 1425

9.7.1.2 TDD 1425

9.7.1.3 FDD (Category 1bis UE) 1426

9.7.1.4 TDD (Category 1bis UE) 1427

9.7.2 CQI reporting under fading conditions 1428

9.7.2.1 FDD and half-duplex FDD 1428

9.7.2.2 TDD 1429

9.7.2.3 FDD (Category 1bis UE) 1430

9.7.2.4 TDD (Category 1bis UE) 1431

9.8 CSI reporting (UE supporting coverage enhancement) 1432

9.8.1 CQI reporting definition under AWGN conditions 1432

9.8.1.1 FDD and half-duplex FDD 1432

9.8.1.2 TDD 1433

9.8.2 UE-selected subband CQI 1434

9.8.2.1 FDD and half-duplex FDD 1434

9.8.2.2 TDD 1438

9.8.3 CQI reporting definition for UE supporting 64QAM under AWGN 1441

9.8.3.1 FDD and half-duplex FDD 1441

9.8.3.2 TDD 1442

9.8.4 CQI reporting definition for UE supporting alternative table under AWGN 1443

9.8.4.1 FDD and half-duplex FDD 1443

9.8.4.2 TDD 1444

9.9 CSI reporting for 4Rx UE 1445

9.9.1 CQI reporting definition under AWGN conditions 1445

9.9.1.1 Minimum requirement PUCCH 1-0 with Rank 1 (Cell-Specific Reference Symbols) 1446

9.9.1.1.1 FDD 1446

9.9.1.1.2 TDD 1446

9.9.1.2 Minimum requirement PUCCH 1-1 with Rank 2 (CSI Reference Symbols) 1447

9.9.1.2.1 FDD 1447

9.9.1.2.2 TDD 1448

9.9.1.3 Minimum requirement PUCCH 1-1 with Rank 4 (Cell-Specific Reference Symbols) 1449

9.9.1.3.1 FDD 1450

9.9.1.3.2 TDD 1450

9.9.1.4 Minimum requirement PUCCH 1-1 with Rank 3 (CSI Reference Symbols) 1451

9.9.1.4.1 FDD 1451

9.9.1.4.2 TDD 1452

9.9.2 CQI reporting definition under fading conditions 1453

9.9.2.1 Minimum requirement PUCCH 1-0 (Cell-Specific Reference Symbol) for enhanced receiver Type A 1453

9.9.2.1.1 FDD 1454

9.9.2.1.2 TDD 1455

9.9.2.2 Minimum requirement PUCCH 1-1 (CSI Reference Symbol) for enhanced receiver Type A 1457

9.9.2.2.1 FDD 1457

9.9.2.2.2 TDD 1460

9.9.3 Reporting of Precoding Matrix Indicator (PMI) for 4Rx UE 1463

9.9.3.1 Minimum requirement PUSCH 3-1 (CSI Reference Symbol) 1464

9.9.3.1.1 TDD 1464

9.9.4 Reporting of Rank Indicator (RI) 1466

9.9.4.1 Minimum requirement (Cell-Specific Reference Symbols) 1466

9.9.4.1.1 FDD 1466

9.9.4.1.2 TDD 1468

9.9.4.2 Minimum requirement (CSI Reference Symbols) 1469

9.9.4.2.1 FDD 1469

9.9.4.2.2 TDD 1471

9.10 Reporting of CSI-RS Resource Indicator (CRI) 1473

9.10.1 Minimum requirement (PUSCH 3-1) 1474

9.10.1.1 FDD 1474

9.10.1.2 TDD 1476

9.10.2 Minimum requirement (PUSCH 3-1, QCL Type C) 1478

9.10.2.1 FDD 1478

9.10.2.2 TDD 1481

9.11 Reporting of Hybrid Channel state information 1484

9.11.1 Minimum requirement (with eMIMO-Type configured as Class B with more than one CSI-RS resource configured and eMIMO-Type2 as Class B with one CSI-RS resource configured) 1484

9.11.1.1 FDD 1485

9.11.1.2 TDD 1487

9.12 CSI reporting (UE supporting Short TTI) 1489

9.12.1 CQI reporting under fading conditions (Cell-Specific Reference Symbol) 1489

9.12.1.1 FDD 1489

9.12.1.2 TDD 1492

9.12.2 CQI reporting under fading conditions (CSI Reference Symbol) 1493

9.12.2.1 FDD 1493

9.12.2.2 TDD 1496

9.13 CSI reporting for 8Rx UE 1498

9.13.1 CQI reporting definition under AWGN conditions 1498

9.13.1.1 Minimum requirement PUCCH 1-1 with Rank 4 (CSI Reference Symbols) 1498

9.13.1.2.1 Void 1498

9.13.1.2.2 TDD 1498

10 Performance requirement (MBMS) 1499

10.1 FDD (Fixed Reference Channel) 1499

10.1.1 Minimum requirement 1500

10.2 TDD (Fixed Reference Channel) 1501

10.2.1 Minimum requirement 1501

10.3 FDD (Fixed Reference Channel) with FeMBMS 1502

10.3.1 Minimum requirement for FeMBMS Unicast-mixed Cell under CA 1502

10.3.1.1 Minimum requirement with 1.25kHz subcarrier spacing 1502

10.3.1.2 Minimum requirement with 7.5kHz subcarrier spacing 1503

10.3.2 Minimum requirement for FeMBMS Unicast-mixed Cell as Non-Serving Cell 1504

10.3.2.1 Minimum requirement with 1.25kHz subcarrier spacing 1504

10.3.2.2 Minimum requirement with 7.5kHz subcarrier spacing 1505

10.3.3 Minimum requirement for MBMS Dedicated cell 1506

10.3.3.1 Minimum requirement with 1.25kHz subcarrier spacing 1506

10.3.3.2 Minimum requirement with 7.5kHz subcarrier spacing 1507

10.3.3.3 Minimum requirement with 15kHz subcarrier spacing 1508

11 Performance requirement (ProSe Direct Discovery) 1509

11.1 General 1509

11.1.1 Applicability of requirements 1509

11.1.2 Reference DRX configuration 1510

11.2 Demodulation of PSDCH (single link performance) 1510

11.2.1 FDD (in-coverage) 1510

11.2.2 TDD (in-coverage) 1511

11.2.3 FDD (out-of-coverage) 1512

11.3 Power imbalance performance with two links 1512

11.3.1 FDD 1512

11.3.2 TDD 1513

11.4 Multiple timing reference test 1514

11.4.1 FDD 1515

11.5 Maximum Sidelink processes test 1516

11.5.1 FDD 1516

11.5.2 TDD 1517

12 Performance requirement (ProSe Direct Communication) 1519

12.1 General 1519

12.1.1 Applicability of requirements 1519

12.1.1.1 Applicability of requirements for different channel bandwidths 1519

12.1.1.2 Test coverage for different number of component carriers 1519

12.1.1.3 Applicability and test rules for different CA configurations and bandwidth combination sets 1519

12.1.2 Reference DRX configuration 1520

12.2 Demodulation of PSSCH 1520

12.2.1 FDD 1520

12.3 Demodulation of PSCCH 1521

12.3.1 FDD 1522

12.4 Demodulation of PSBCH 1523

12.4.1 FDD 1523

12.5 Power imbalance performance with two links 1523

12.5.1 FDD 1523

12.6 Multiple timing reference test 1525

12.6.1 FDD 1525

12.7 Maximum Sidelink processes test 1528

12.7.1 FDD 1528

12.8 Sustained downlink data rate with active Sidelink 1529

13 Void 1531

14 Performance requirement (V2X Sidelink Communication) 1531

14.1 General 1531

14.1.1 Applicability of requirements 1531

14.2 Demodulation of PSSCH 1532

14.3 Demodulation of PSCCH 1533

14.4 Power imbalance performance with two links 1533

14.5 Demodulation of PSBCH 1534

14.6 Demodulation of PSSCH with eNB based synchronization 1535

14.7 Soft buffer test 1535

14.8 PSCCH decoding capability test 1536

14.9 Sustained downlink data rate with active sidelink 1537

14.10 Soft buffer test (CA) 1538

14.11 PSCCH/PSSCH decoding capability test (CA) 1539

Annex A (normative): Measurement channels 1542

A.1 General 1542

A.2 UL reference measurement channels 1542

A.2.1 General 1542

A.2.1.1 Applicability and common parameters 1542

A.2.1.2 Determination of payload size 1542

A.2.1.3 Overview of UL reference measurement channels 1543

A.2.2 Reference measurement channels for FDD 1566

A.2.2.1 Full RB allocation 1566

A.2.2.1.1 QPSK 1566

A.2.2.1.2 16-QAM 1568

A.2.2.1.3 64-QAM 1570

A.2.2.1.4 256 QAM 1571

A.2.2.2 Partial RB allocation 1571

A.2.2.2.1 QPSK 1572

A.2.2.2.2 16-QAM 1575

A.2.2.2.3 64-QAM 1577

A.2.2.2.4 256 QAM 1579

A.2.2.3 Void 1579

A.2.2.4 subPRB allocation 1580

A.2.3 Reference measurement channels for TDD 1580

A.2.3.1 Full RB allocation 1580

A.2.3.1.1 QPSK 1580

A.2.3.1.2 16-QAM 1583

A.2.3.1.3 64-QAM 1586

A.2.3.1.4 256 QAM 1586

A.2.3.2 Partial RB allocation 1586

A.2.3.2.1 QPSK 1587

A.2.3.2.2 16-QAM 1591

A.2.3.2.3 64-QAM 1596

A.2.3.2.4 256 QAM 1598

A.2.3.3 Void 1598

A.2.3.4 subPRB allocation 1599

A.2.4 Reference measurement channels for UE category NB1 1599

A.2.5 Reference measurement channels for LAA 1600

A.2.5.1 Full RB allocation 1600

A.2.5.1.1 QPSK 1600

A.2.5.1.2 16QAM 1601

A.2.5.1.3 64QAM 1601

A.2.5.2 Partial RB allocation 1601

A.2.5.2.1 QPSK 1602

A.2.5.2.2 16QAM 1602

A.2.5.2.3 64QAM 1603

A.3 DL reference measurement channels 1603

A.3.1 General 1603

A.3.1.1 Overview of DL reference measurement channels 1604

A.3.2 Reference measurement channel for receiver characteristics 1628

A.3.3 Reference measurement channels for PDSCH performance requirements (FDD) 1658

A.3.3.1 Single-antenna transmission (Common Reference Symbols) 1658

A.3.3.2 Multi-antenna transmission (Common Reference Symbols) 1663

A.3.3.2.1 Two antenna ports 1663

A.3.3.2.2 Four antenna ports 1670

A.3.3.3 Reference Measurement Channel for UE-Specific Reference Symbols 1675

A.3.3.3.0 Two antenna ports (no CSI-RS) 1675

A.3.3.3.1 Two antenna port (CSI-RS) 1676

A.3.3.3.2 Four antenna ports (CSI-RS) 1679

A.3.3.3.2A Eight antenna ports (CSI-RS) 1686

A.3.3.3.3 Twelve antenna port (CSI-RS) 1687

A.3.3.3.4 Sixteen antenna port (CSI-RS) 1688

A.3.3.3.5 Twenty-four antenna port (CSI-RS) 1689

A.3.3.3.6 Thirty-two antenna port (CSI-RS) 1690

A.3.4 Reference measurement channels for PDSCH performance requirements (TDD) 1692

A.3.4.1 Single-antenna transmission (Common Reference Symbols) 1692

A.3.4.2 Multi-antenna transmission (Common Reference Signals) 1700

A.3.4.2.1 Two antenna ports 1700

A.3.4.2.2 Four antenna ports 1713

A.3.4.3 Reference Measurement Channels for UE-Specific Reference Symbols 1720

A.3.4.3.1 Single antenna port (Cell Specific) 1720

A.3.4.3.2 Two antenna ports (Cell Specific) 1721

A.3.4.3.3 Two antenna ports (CSI-RS) 1723

A.3.4.3.4 Four antenna ports (CSI-RS) 1731

A.3.4.3.5 Eight antenna ports (CSI-RS) 1738

A.3.4.3.6 Twelve antenna ports (CSI-RS) 1743

A.3.4.3.7 Sixteen antenna ports (CSI-RS) 1744

A.3.4.3.8 Twenty-four antenna ports (CSI-RS) 1745

A.3.4.3.9 Thirty-two antenna ports (CSI-RS) 1746

A.3.5 Reference measurement channels for PDCCH/PCFICH performance requirements 1748

A.3.5.1 FDD 1748

A.3.5.2 TDD 1748

A.3.5.3 LAA 1749

A.3.6 Reference measurement channels for PHICH performance requirements 1749

A.3.7 Reference measurement channels for PBCH performance requirements 1749

A.3.8 Reference measurement channels for MBMS performance requirements 1750

A.3.8.1 FDD 1750

A.3.8.2 TDD 1754

A.3.9 Reference measurement channels for sustained downlink data rate provided by lower layers 1756

A.3.9.1 FDD 1756

A.3.9.2 TDD 1760

A.3.9.3 FDD (EPDCCH scheduling) 1774

A.3.9.4 TDD (EPDCCH scheduling) 1775

A.3.9.5 LAA 1777

A.3.10 Reference Measurement Channels for EPDCCH performance requirements 1779

A.3.10.1 FDD 1779

A.3.10.2 TDD 1779

A.3.11 Reference Measurement Channels for MPDCCH performance requirements 1779

A.3.11.1 FDD and half-duplex FDD 1779

A.3.11.2 TDD 1780

A.3.12 Reference measurement channels for NPDSCH performance requirements 1781

A.3.12.1 In-band 1781

A.3.12.1.2 Two-antenna transmission 1781

A.3.12.2 Standalone/Guard-band 1783

A.3.12.2.1 Single-antenna transmission 1783

A.3.13 Reference measurement channels for NPDCCH performance requirements 1786

A.3.13.1 Half-duplex FDD 1786

A.3.13.2 TDD 1787

A.3.14 Reference measurement channels for NPBCH performance requirements for Cat NB1 UEs 1787

A.3.15 Reference Measurement Channels for LAA SCell with frame structure Type-3 1788

A.3.15.1 Multi-antenna transmission (Common Reference Symbols) 1788

A.3.15.1.1 Four antenna ports 1788

A.3.15.2 Reference Measurement Channel for UE-Specific Reference Symbols 1788

A.3.15.2.1 Two antenna ports (CSI-RS) 1788

A.3.16 Reference measurement channels for Slot-PDSCH and Subslot-PDSCH performance requirements 1790

A.3.16.1 FDD 1790

A.3.16.2 TDD 1794

A.3.17 Reference measurement channels for SPDCCH performance requirements 1795

A.3.17.1 FDD 1795

A.3.17.2 TDD 1796

A.4 CSI reference measurement channels 1796

A.5 OFDMA Channel Noise Generator (OCNG) 1811

A.5.1 OCNG Patterns for FDD 1811

A.5.1.1 OCNG FDD pattern 1: One sided dynamic OCNG FDD pattern 1811

A.5.1.2 OCNG FDD pattern 2: Two sided dynamic OCNG FDD pattern 1812

A.5.1.3 OCNG FDD pattern 3: 49 RB OCNG allocation with MBSFN in 10 MHz 1812

A.5.1.3A OCNG FDD pattern 3A: 49 RB OCNG allocation with MBSFN enhancement in 10 MHz 1813

A.5.1.4 OCNG FDD pattern 4: One sided dynamic OCNG FDD pattern for MBMS transmission 1813

A.5.1.4A OCNG FDD pattern 4A: One sided dynamic OCNG FDD pattern for enhanced MBMS transmission 1814

A.5.1.5 OCNG FDD pattern 5: One sided dynamic 16QAM modulated OCNG FDD pattern 1815

A.5.1.6 OCNG FDD pattern 6: dynamic OCNG FDD pattern when user data is in 2 non-contiguous blocks 1816

A.5.1.8 OCNG FDD pattern 8: Dynamic OCNG FDD pattern for TM10 transmission 1817

A.5.2 OCNG Patterns for TDD 1818

A.5.2.1 OCNG TDD pattern 1: One sided dynamic OCNG TDD pattern 1818

A.5.2.2 OCNG TDD pattern 2: Two sided dynamic OCNG TDD pattern 1819

A.5.2.3 OCNG TDD pattern 3: 49 RB OCNG allocation with MBSFN in 10 MHz 1820

A.5.2.4 OCNG TDD pattern 4: One sided dynamic OCNG TDD pattern for MBMS transmission 1820

A.5.2.5 OCNG TDD pattern 5: One sided dynamic 16QAM modulated OCNG TDD pattern 1821

A.5.2.6 OCNG TDD pattern 6: dynamic OCNG TDD pattern when user data is in 2 non-contiguous blocks 1822

A.5.2.8 OCNG TDD pattern 8: Dynamic OCNG TDD pattern for TM10 transmission 1823

A.5.3 OCNG Patterns for Narrowband IoT 1824

A.5.3.1 Narrowband IoT OCNG pattern 1 1824

A.5.4 OCNG Patterns for frame structure type 3 1825

A.5.4.1 OCNG FS3 pattern 1: One sided dynamic OCNG frame structure type 3 pattern 1825

A.5.4.2 OCNG FS3 pattern 2: Two sided dynamic OCNG frame structure 3 pattern 1826

A.6 Sidelink reference measurement channels 1827

A.6.1 General 1827

A.6.1.1 Overview of ProSe reference measurement channels 1827

A.6.2 Reference measurement channel for receiver characteristics 1828

A.6.3 Reference measurement channels for PSDCH performance requirements 1830

A.6.4 Reference measurement channels for PSCCH performance requirements 1831

A.6.5 Reference measurement channels for PSSCH performance requirements 1831

A.6.6 Reference measurement channels for PSBCH performance requirements 1832

A.7 Sidelink reference resource pool configurations 1833

A.7.1 Reference resource pool configurations for ProSe Direct Discovery demodulation tests 1833

A.7.1.1 FDD 1833

A.7.1.2 TDD 1836

A.7.2 Reference resource pool configurations for ProSe Direct Communication demodulation tests 1838

A.7.2.1 FDD 1838

A.8 V2X reference measurement channels 1843

A.8.1 General 1843

A.8.1.1 Overview of V2X reference measurement channels 1844

A.8.2 Reference measurement channel for receiver characteristics 1844

A.8.3 Reference measurement channel for transmitter characteristics 1846

A.8.4 Reference measurement for PSCCH performance requirements 1849

A.8.5 Reference measurement for PSSCH performance requirements 1850

A.8.6 Reference measurement for PSBCH performance requirements 1850

A.9 V2X reference resource pool configurations 1851

Annex B (normative): Propagation conditions 1854

B.1 Static propagation condition 1854

B.1.1 UE Receiver with 2Rx 1854

B.1.2 UE Receiver with 4Rx 1854

B.1.3 UE Receiver with 8Rx 1855

B.2 Multi-path fading propagation conditions 1856

B.2.1 Delay profiles 1856

B.2.2 Combinations of channel model parameters 1857

B.2.3 MIMO Channel Correlation Matrices 1858

B.2.3.1 Definition of MIMO Correlation Matrices 1858

B.2.3.2 MIMO Correlation Matrices at High, Medium and Low Level 1864

B.2.3A MIMO Channel Correlation Matrices using cross polarized antennas 1867

B.2.3A.1 Definition of MIMO Correlation Matrices using cross polarized antennas 1868

B.2.3A.2 Spatial Correlation Matrices using cross polarized antennas at eNB and UE sides 1868

B.2.3A.2.1 Spatial Correlation Matrices at eNB side 1868

B.2.3A.2.2 Spatial Correlation Matrices at UE side 1869

B.2.3A.4 Beam steering approach 1872

B.2.3B MIMO Channel Correlation Matrices using two-dimension cross polarized antennas at eNB and cross polarized antennas at UE 1872

B.2.3B.1 Definition of MIMO Correlation Matrices using two-dimension cross polarized antennas at eNB and cross polarized antennas at UE 1873

B.2.3B.2 Spatial Correlation Matrices using two-dimension cross polarized antennas at eNB and cross polarized antennas at UE 1874

B.2.3B.2.1 Spatial Correlation Matrices at eNB side 1874

B.2.3B.2.2 Spatial Correlation Matrices at UE side 1874

B.2.3B.3 MIMO Correlation Matrices using two-dimension cross polarized antennas at eNB and cross polarized antennas at UE 1874

B.2.3B.4 Beam steering approach 1877

B.2.3B.4A Beam steering approach with dual cluster beams 1878

B.2.4 Propagation conditions for CQI tests 1879

B.2.4.1 Propagation conditions for CQI tests with multiple CSI processes 1879

B.2.5 Void 1879

B.2.6 MBSFN Propagation Channel Profile 1879

B.2.6.1 Subcarrier spacing 15kHz or 7.5kHz 1879

B.2.6.2 Subcarrier spacing 1.25kHz 1880

B.3 High speed train scenario 1881

B.3A HST-SFN scenario 1882

B.4 Beamforming Model 1886

B.4.1 Single-layer random beamforming (Antenna port 5, 7, or 8) 1886

B.4.1A Single-layer random beamforming (Antenna port 7, 8, 11 or 13 with enhanced DMRS table configured) 1886

B.4.2 Dual-layer random beamforming (antenna ports 7 and 8) 1887

B.4.3 Generic beamforming model (antenna ports 7-14) 1887

B.4.4 Random beamforming for EPDCCH distributed transmission (Antenna port 107 and 109) 1888

B.4.5 Random beamforming for EPDCCH localized transmission (Antenna port 107, 108, 109 or 110) 1888

B.4.6 Beamforming model for CRI test 1888

B.5 Interference models for enhanced performance requirements Type-A 1890

B.5.1 Dominant interferer proportion 1890

B.5.2 Transmission mode 3 interference model 1890

B.5.3 Transmission mode 4 interference model 1891

B.5.4 Transmission mode 9 interference model 1891

B.6 Interference models for enhanced performance requirements Type-B 1891

B.6.1 Transmission mode 2 interference model 1892

B.6.2 Transmission mode 3 interference model 1892

B.6.3 Transmission mode 4 interference model 1892

B.6.4 Transmission mode 9 interference model 1893

B.6.5 CRS interference model 1893

B.6.6 Random interference model 1893

B.7 Interference models for enhanced downlink control channel performance requirements Type A and B 1894

B.7.1 PDCCH, PCFICH and PHICH interference model 1894

B.8 Burst transmission models for Frame structure type 3 1895

B.8.1 Burst transmission model for one LAA SCell 1895

B.8.2 Burst transmission model for multiple LAA SCell(s) 1896

Annex C (normative): Downlink Physical Channels 1897

C.1 General 1897

C.2 Set-up 1897

C.3 Connection 1897

C.3.1 Measurement of Receiver Characteristics 1897

C.3.2 Measurement of Performance requirements 1898

C.3.3 Aggressor cell power allocation for Measurement of Performance Requirements when ABS is Configured 1899

C.3.4 Power Allocation for Measurement of Performance Requirements when Quasi Co-location Type B: same Cell ID 1900

C.3.5 Simplified CA testing method 1900

C.3.6 Measurement of Receiver Characteristics for Narrowband IoT 1901

Annex D (normative): Characteristics of the interfering signal 1902

D.1 General 1902

D.2 Interference signals 1902

Annex E (normative): Environmental conditions 1903

E.1 General 1903

E.2 Environmental 1903

E.2.1 Temperature 1903

E.2.2 Voltage 1903

E.2.3 Vibration 1904

Annex F (normative): Transmit modulation 1905

F.1 Measurement Point 1905

F.2 Basic Error Vector Magnitude measurement 1905

F.3 Basic in-band emissions measurement 1906

F.4 Modified signal under test 1906

F.5 Window length 1908

F.5.1 Timing offset 1908

F.5.2 Window length 1908

F.5.3 Window length for normal CP 1908

F.5.4 Window length for Extended CP 1909

F.5.5 Window length for PRACH 1909

F.5.F Window length for category NB1 1910

F.6 Averaged EVM 1910

F.6.F Averaged EVM for category NB1 1911

F.7 Spectrum Flatness 1911

Annex G (informative): Reference sensitivity level in lower SNR 1912

G.1 General 1912

G.2 Typical receiver sensitivity performance (QPSK) 1912

G.3 Reference measurement channel for REFSENSE in lower SNR 1918

Annex H (normative): Modified MPR behavior 1921

H.1 Indication of modified MPR behavior 1921

Annex I (normative): Supported Post Antenna Gain 1922

I.1 Declared Supported Post Antenna Gain for UE 1922

Annex J (informative): Change history 1923