|  |  |
| --- | --- |
| 3GPP TS 38.101-1 V17.8.0 (2022-12) | |
| Technical Specification | |
| 3rd Generation Partnership Project;  Technical Specification Group Radio Access Network;  NR;  User Equipment (UE) radio transmission and reception;  Part 1: Range 1 Standalone  (Release 17) | |
|  | |
|  |  |
|  | |
| The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP. The present document has not been subject to any approval process by the 3GPPOrganizational Partners and shall not be implemented. This Specification is provided for future development work within 3GPPonly. The Organizational Partners accept no liability for any use of this Specification. Specifications and Reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organizational Partners' Publications Offices. | |

|  |
| --- |
|  |
| ***3GPP***  Postal address  3GPP support office address  650 Route des Lucioles - Sophia Antipolis  Valbonne - FRANCE  Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16  Internet  http://www.3gpp.org |
| ***Copyright Notification***  No part may be reproduced except as authorized by written permission. The copyright and the foregoing restriction extend to reproduction in all media.  © 2022, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).  All rights reserved.  UMTS™ is a Trade Mark of ETSI registered for the benefit of its members  3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  GSM® and the GSM logo are registered and owned by the GSM Association |

Contents

Foreword 16

1 Scope 18

2 References 18

3 Definitions, symbols and abbreviations 19

3.1 Definitions 19

3.2 Symbols 20

3.3 Abbreviations 22

4 General 23

4.1 Relationship between minimum requirements and test requirements 23

4.2 Applicability of minimum requirements 23

4.3 Specification suffix information 23

5 Operating bands and channel arrangement 25

5.1 General 25

5.2 Operating bands 25

5.2A Operating bands for CA 27

5.2A.0 General 27

5.2A.1 Intra-band CA 27

5.2A.2 Inter-band CA 28

5.2A.2.1 Inter-band CA (two bands) 29

5.2A.2.2 Inter-band CA (three bands) 35

5.2A.2.3 Inter-band CA (four bands) 40

5.2A.2.4 Inter-band CA (five bands) 42

5.2B Operating bands for DC 42

5.2C Operating band combination for SUL 42

5.2D Operating bands for UL MIMO 44

5.2E Operating band for V2X 45

5.2E.1 V2X operating bands 45

5.2E.2 V2X operating bands for con-current operation 45

5.3 UE channel bandwidth 46

5.3.1 General 46

5.3.2 Maximum transmission bandwidth configuration 48

5.3.3 Minimum guardband and transmission bandwidth configuration 48

5.3.4 RB alignment 50

5.3.5 UE channel bandwidth per operating band 50

5.3.6 Asymmetric channel bandwidths 54

5.3A UE channel bandwidth for CA 55

5.3A.1 General 55

5.3A.2 Maximum transmission bandwidth configuration for CA 56

5.3A.3 Minimum guardband and transmission bandwidth configuration for CA 56

5.3A.4 Void 57

5.3A.5 UE channel bandwidth per operating band for CA 57

5.3E Channel bandwidth for V2X 58

5.3E.1 General 58

5.3E.2 Channel bandwidth for V2X concurrent operation 60

5.3I Channel bandwidth for RedCap 61

5.4 Channel arrangement 61

5.4.1 Channel spacing 61

5.4.1.1 Channel spacing for adjacent NR carriers 61

5.4.2 Channel raster 61

5.4.2.1 NR-ARFCN and channel raster 61

5.4.2.2 Channel raster to resource element mapping 62

5.4.2.3 Channel raster entries for each operating band 62

5.4.3 Synchronization raster 66

5.4.3.1 Synchronization raster and numbering 66

5.4.3.3 Synchronization raster entries for each operating band 67

5.4.4 TX–RX frequency separation 70

5.4A Channel arrangement for CA 71

5.4A.1 Channel spacing for CA 71

5.4A.2 Channel raster for CA 72

5.4A.3 Synchronization raster for CA 72

5.4A.4 Tx-Rx frequency separation for CA 72

5.4B Reserved 72

5.4C Reserved 72

5.4D Reserved 72

5.4E Channel arrangement for V2X 72

5.4E.1 Channel spacing 72

5.4E.2 Channel raster 73

5.4E.2.1 NR-ARFCN and channel raster 73

5.4E.2.2 Channel raster to resource element mapping 73

5.4E.2.3 Channel raster entries for each operating band 73

5.4E.3 Synchronization raster for V2X 73

5.5 Void 73

5.5A Configurations for CA 73

5.5A.0 General 73

5.5A.1 Configurations for intra-band contiguous CA 74

5.5A.2 Configurations for intra-band non-contiguous CA 79

5.5A.3 Configurations for inter-band CA 83

5.5A.3.1 Configurations for inter-band CA (two bands) 83

5.5A.3.2 Configurations for inter-band CA (three bands) 119

5.5A.3.3 Configurations for inter-band CA (four bands) 181

5.5A.3.4 Configurations for inter-band CA (five bands) 215

5.5B Configurations for DC 218

5.5C Configurations for SUL 224

6 Transmitter characteristics 231

6.1 General 231

6.1A General 231

6.1F General 231

6.2 Transmitter power 231

6.2.1 UE maximum output power 231

6.2.1I Void 233

6.2.2 UE maximum output power reduction 233

6.2.3 UE additional maximum output power reduction 236

6.2.3.1 General 236

6.2.3.2 A-MPR for NS\_04 241

6.2.3.3 A-MPR for NS\_10 242

6.2.3.4 A-MPR for NS\_05 and NS\_05U 242

6.2.3.5 A-MPR for NS\_40 246

6.2.3.6 A-MPR for NS\_43 and NS\_43U 247

6.2.3.7 A-MPR for NS\_03 and NS\_03U 248

6.2.3.8 A-MPR for NS\_37 248

6.2.3.9 A-MPR for NS\_38 249

6.2.3.10 A-MPR for NS\_39 249

6.2.3.11 A-MPR for NS\_41 250

6.2.3.12 A-MPR for NS\_42 250

6.2.3.13 A-MPR for NS\_18 251

6.2.3.14 A-MPR for NS\_21 252

6.2.3.15 A-MPR for NS\_24 253

6.2.3.16 A-MPR for NS\_27 254

6.2.3.17 A-MPR for NS\_46 255

6.2.3.18 A-MPR for NS\_47 256

6.2.3.19 A-MPR for NS\_50 257

6.2.3.20 A-MPR for NS\_44 259

6.2.3.21 A-MPR for NS\_12 259

6.2.3.22 A-MPR for NS\_13 260

6.2.3.23 A-MPR for NS\_14 260

6.2.3.24 A-MPR for NS\_15 261

6.2.3.25 A-MPR for NS\_45 262

6.2.3.26 A-MPR for NS\_48 262

6.2.3.27 A-MPR for NS\_49 264

6.2.3.28 A-MPR for NS\_51 266

6.2.3.29 A-MPR for NS\_07 267

6.2.3.30 A-MPR for NS\_56 267

6.2.4 Configured transmitted power 268

6.2A Transmitter power for CA 271

6.2A.1 UE maximum output power for CA 271

6.2A.1.1 UE maximum output power for Intra-band contiguous CA 271

6.2A.1.2 UE maximum output power for Intra-band non-contiguous CA 271

6.2A.1.3 UE maximum output power for Inter-band CA 271

6.2A.1.4 Void 277

6.2A.1.5 Void 277

6.2A.2 UE maximum output power reduction for CA 277

6.2A.2.1 UE maximum output power reduction for Intra-band contiguous CA 277

6.2A.2.2 UE maximum output power reduction for Intra-band non-contiguous CA 280

6.2A.2.2.0 General 280

6.2A.2.2.1 MPR to meet -30dBm/MHz 281

6.2A.2.2.1.1 PC3 with indicating dualPA-Architecture supported 281

6.2A.2.2.1.2 PC2 with indicating dualPA-Architecture supported 282

6.2A.2.2.1.3 PC3 without indicating dualPA-Architecture supported 282

6.2A.2.2.1.4 PC2 without indicating dualPA-Architecture supported 282

6.2A.2.2.2 MPR to meet -13dBm/MHz 283

6.2A.2.2.2.1 PC3 with indicating dualPA-Architecture supported 283

6.2A.2.2.2.2 PC2 with indicating dualPA-Architecture supported 283

6.2A.2.2.2.3 PC3 without indicating dualPA-Architecture supported 283

6.2A.2.2.2.4 PC2 without indicating dualPA-Architecture supported 284

6.2A.2.3 UE maximum output power reduction for Inter-band CA 284

6.2A.2.4 Void 284

6.2A.3 UE additional maximum output power reduction for CA 284

6.2A.3.1 UE additional maximum output power reduction for Intra-band CA 284

6.2A.3.1.1 UE additional maximum output power reduction for Intra-band contiguous CA 284

6.2A.3.1.1.1 A-MPR for CA\_NS\_04 285

6.2A.3.1.1.1.2 Non-contiguous allocations 286

6.2A.3.1.2 UE additional maximum output power reduction for Intra-band non-contiguous CA 291

6.2A.3.1.3 UE additional maximum output power reduction for Inter-band CA 294

6.2A.4 Configured output power for CA 298

6.2A.4.1 Configured transmitted power level 298

6.2A.4.1.1 Configured transmitted power for Intra-band contiguous CA 298

6.2A.4.1.2 Configured transmitted power for Intra-band non-contiguous CA 300

6.2A.4.1.3 Configured transmitted power for Inter-band CA 303

6.2A.4.1.4 Void 306

6.2A.4.2 ΔTIB,c for CA 306

6.2A.4.2.1 Void 306

6.2A.4.2.2 Void 306

6.2A.4.2.3 ΔTIB,c for Inter-band CA (two bands) 306

6.2A.4.2.4 ΔTIB,c for Inter-band CA (three bands) 314

6.2A.4.2.5 ΔTIB,c for Inter-band CA (four bands) 324

6.2A.4.2.6 ΔTIB,c for Inter-band CA (five bands) 330

6.2B Transmitter power for NR-DC 330

6.2B.0 General 330

6.2B.1 UE maximum output power for NR-DC 330

6.2B.2 UE maximum output power reduction for NR-DC 331

6.2B.3 UE additional maximum output power reduction for NR-DC 331

6.2B.4.1 Configured transmitted power level for NR-DC 332

6.2B.4.2 ΔTIB,c for NR-DC 336

6.2C Transmitter power for SUL 336

6.2C.1 Configured transmitted power for SUL 336

6.2C.2 ΔTIB,c 337

6.2D Transmitter power for UL MIMO 339

6.2D.1 UE maximum output power for UL MIMO 339

6.2D.2 UE maximum output power reduction for UL MIMO 340

6.2D.3 UE additional maximum output power reduction for UL MIMO 341

6.2D.4 Configured transmitted power for UL MIMO 342

6.2E Transmitter power for V2X 342

6.2E.1 UE maximum output power for V2X 342

6.2E.1.1 General 342

6.2E.1.2 UE maximum output power for V2X con-current operation 343

6.2E.2 UE maximum output power reduction for V2X 344

6.2E.2.1 General 344

6.2E.2.2 MPR for Power class 2 and Power class 3 V2X UE 344

6.2E.2.3 MPR for Power class 2 and Power class 3 V2X con-current operation 346

6.2E.2.4 MPR for Power class 1 UE in Band n14 349

6.2E.3 UE additional maximum output power reduction for V2X 349

6.2E.3.1 General 349

6.2E.3.2 A-MPR for V2X UE by NS\_33 350

6.2E.3.3 A-MPR for Power class 3 V2X UE by NS\_52 353

6.2E.3.4 A-MPR for V2X con-current operation 354

6.2E.4 Configured transmitted power for V2X 355

6.2E.4.1 General 355

6.2E.4.2 Configured transmitted power for inter-band V2X con-current operation 356

6.2E.4.3 Configured transmitted power for intra-band V2X con-current operation 356

6.2F Transmitter power for shared spectrum channel access 359

6.2F.1 UE maximum output power 359

6.2F.1A UE maximum output power for CA 360

6.2F.1A.1 UE maximum output power for inter-band CA 360

6.2F.1A.2 UE maximum output power for intra-band contiguous CA 360

6.2F.1B UE maximum output power for NR-DC 360

6.2F.1D UE maximum output power for UL MIMO 360

6.2F.2 UE maximum output power reduction 361

6.2F.2A UE maximum output power reduction for CA 362

6.2F.2A.1 UE maximum output power reduction for inter-band CA 362

6.2F.2A.2 UE maximum output power reduction for intra-band contiguous CA 362

6.2F.2D UE maximum output power reduction for UL MIMO 364

6.2F.3 UE additional maximum output power reduction 365

6.2F.3.1 General 365

6.2F.3.2 A-MPR for NS\_28 366

6.2F.3.3 A-MPR for NS\_29 366

6.2F.3.4 A-MPR for NS\_30 367

6.2F.3.5 A-MPR for NS\_31 367

6.2F.3.6 A-MPR for NS\_53 368

6.2F.3.7 A-MPR for NS\_54 368

6.2F.3.8 A-MPR for NS\_58 369

6.2F.3.9 A-MPR for NS\_59 370

6.2F.3.10 A-MPR for NS\_60 371

6.2F.3.11 A-MPR for NS\_61 371

6.2F.3A UE additional maximum output power reduction for CA 372

6.2F.3A.1 UE additional maximum output power reduction for inter-band CA 372

6.2F.3D UE additional maximum output power reduction for UL MIMO 372

6.2F.4 Configured transmitted power 372

6.2F.4D Configured transmitted power UL MIMO 372

6.2G Transmitter power for Tx Diversity 373

6.2G.1 UE maximum output power for Tx Diversity 373

6.2G.2 UE maximum output power reduction for Tx Diversity 373

6.2G.3 UE additional maximum output power reduction for Tx Diversity 373

6.2G.4 Configured transmitted power for Tx Diversity 373

6.2H Transmitter power for CA with UL MIMO 374

6.2H.1 Transmitter power for intra-band UL contiguous CA with UL MIMO 374

6.2H.1.1 UE maximum output power for intra-band UL contiguous CA with UL MIMO 374

6.2H.1.2 UE maximum output power reduction for intra-band UL contiguous CA with UL MIMO 374

6.2H.1.3 UE additional maximum output power reduction for intra-band UL contiguous CA with UL MIMO 375

6.2H.1.4 Configured transmitted power for intra-band UL contiguous CA with UL MIMO 375

6.2I Transmitter power for RedCap 375

6.2I.1 Maximum output power for RedCap 375

6.3 Output power dynamics 376

6.3.1 Minimum output power 376

6.3.2 Transmit OFF power 376

6.3.3 Transmit ON/OFF time mask 376

6.3.3.1 General 376

6.3.3.2 General ON/OFF time mask 377

6.3.3.3 Transmit power time mask for slot and short or long subslot boundaries 377

6.3.3.4 PRACH time mask 377

6.3.3.5 Void 379

6.3.3.6 SRS time mask 379

6.3.3.7 PUSCH-PUCCH and PUSCH-SRS time masks 380

6.3.3.8 Transmit power time mask for consecutive slot or long subslot transmission and short subslot transmission boundaries 381

6.3.3.9 Transmit power time mask for consecutive short subslot transmissions boundaries 382

6.3.4 Power control 383

6.3.4.1 General 383

6.3.4.2 Absolute power tolerance 383

6.3.4.3 Relative power tolerance 383

6.3.4.4 Aggregate power tolerance 384

6.3A Output power dynamics for CA 384

6.3A.1 Minimum output power for CA 384

6.3A.1.1 Minimum output power for intra-band contiguous CA 384

6.3A.1.2 Minimum output power for intra-band non-contiguous CA 384

6.3A.1.3 Minimum output power for inter-band CA 384

6.3A.1.4 Void 385

6.3A.2 Transmit OFF power for CA 385

6.3A.2.1 Transmit OFF power for intra-band contiguous CA 385

6.3A.2.2 Transmit OFF power for intra-band non-contiguous CA 385

6.3A.2.3 Transmit OFF power for inter-band CA 385

6.3A.2.4 Void 385

6.3A.3 Transmit ON/OFF time mask for CA 385

6.3A.3.1 Transmit ON/OFF time mask for intra-band contiguous CA 385

6.3A.3.2 Transmit ON/OFF time mask for intra-band non-contiguous CA 386

6.3A.3.3 Transmit ON/OFF time mask for inter-band CA 386

6.3A.3.3.1 General 386

6.3A.3.3.2 Time mask for switching between two uplink carriers 386

6.3A.3.3.3 Time mask for switching between two uplink carriers with two transmit antenna connectors 387

6.3A.3.3.4 Time mask for switching between one uplink band with one transmit antenna connector and one uplink band with two transmit antenna connectors 388

6.3A.3.3.5 Time mask for switching between two uplink bands with two transmit antenna connectors 389

6.3A.3.4 Void 390

6.3A.4 Power control for CA 390

6.3A.4.1 Power control for intra-band contiguous CA 390

6.3A.4.1.1 Absolute power tolerance 390

6.3A.4.1.2 Relative power tolerance 390

6.3A.4.1.3 Aggregate power control tolerance 391

6.3A.4.2 Power control for intra-band non-contiguous CA 391

6.3A.4.2.1 Absolute power tolerance 391

6.3A.4.2.1.1 Minimum requirements 391

6.3A.4.2.2 Relative power tolerance 391

6.3A.4.2.2.1 Minimum requirements 391

6.3A.4.2.3 Aggregate power control tolerance 391

6.3A.4.3 Power control for inter-band CA 391

6.3A.4.4 Void 391

6.3B Output power dynamics for NR-DC 391

6.3C Output power dynamics for SUL 392

6.3C.1 Void 392

6.3C.2 Void 392

6.3C.3 Transmit ON/OFF time mask for SUL 392

6.3C.3.1 Time mask for switching between two uplink carriers 392

6.3C.3.2 Time mask for switching between two uplink carriers with two transmit antenna connectors 393

6.3C.3.3 Time mask for switching between one uplink band with one transmit antenna connector and one uplink band with two transmit antenna connectors 393

6.3C.3.4 Time mask for switching between two uplink bands with two transmit antenna connectors 394

6.3D Output power dynamics for UL MIMO 395

6.3D.1 Minimum output power for UL MIMO 395

6.3D.2 Transmit OFF power for UL MIMO 395

6.3D.3 Transmit ON/OFF time mask for UL MIMO 395

6.3D.4 Power control for UL MIMO 396

6.3E Output power dynamics for V2X 396

6.3E.1 Minimum output power for V2X 396

6.3E.1.1 General 396

6.3E.1.2 Minimum output power for V2X con-current operation 396

6.3E.2 Transmit OFF power for V2X 397

6.3E.2.1 General 397

6.3E.2.2 Transmit OFF power for V2X con-current operation 397

6.3E.3 Transmit ON/OFF time mask for V2X 397

6.3E.3.1 General 397

6.3E.3.2 General time mask 397

6.3E.3.3 S-SSB time mask 398

6.3E.3.4 Transmit ON/OFF time mask for V2X con-current operation 398

6.3E.4 Power control for V2X 399

6.3E.4.1 General 399

6.3E.4.2 Absolute power tolerance 400

6.3E.4.3 Power control for V2X con-current operation 400

6.3F Output power dynamics for shared spectrum channel access 400

6.3F.1 Minimum output power 400

6.3F.2 Transmit OFF power 400

6.3F.3 Transmit ON/OFF time mask 400

6.3F.3.1 General 400

6.3F.3.2 General ON/OFF time mask 400

6.3F.3A General ON/OFF mask for CA 401

6.3F.3A.1 General ON/OFF mask for inter-band CA 401

6.3F.4 Power control 401

6.3F.4.1 General 401

6.3F.4.2 Absolute power tolerance 401

6.3F.4.3 Relative power tolerance 401

6.3F.4.4 Aggregate power tolerance 401

6.3F.4A Power control for inter-band CA 401

6.3G Output power dynamics for Tx Diversity 402

6.3G.1 Minimum output power for Tx Diversity 402

6.3G.2 Transmit OFF power for Tx Diversity 402

6.3G.3 Transmit ON/OFF time mask for Tx Diversity 402

6.3G.4 Power control for Tx Diversity 402

6.3H Output power dynamics for CA with UL MIMO 402

6.3H.1 Output power dynamics for intra-band UL contiguous CA with UL MIMO 402

6.3H.1.1 Minimum output power for intra-band UL contiguous CA with UL MIMO 402

6.3H.1.2 Transmit OFF power for intra-band UL contiguous CA with UL MIMO 402

6.3H.1.3 Transmit ON/OFF time mask for intra-band UL contiguous CA with UL MIMO 402

6.3H.1.4 Power control for intra-band UL contiguous CA with UL MIMO 403

6.4 Transmit signal quality 403

6.4.1 Frequency error 403

6.4.2 Transmit modulation quality 403

6.4.2.0 General 403

6.4.2.1 Error Vector Magnitude 403

6.4.2.1a Error Vector Magnitude including symbols with transient period 404

6.4.2.2 Carrier leakage 405

6.4.2.3 In-band emissions 405

6.4.2.4 EVM equalizer spectrum flatness 406

6.4.2.4.1 Requirements for Pi/2 BPSK modulation 407

6.4.2.5 Phase continuity requirements for DMRS bundling 408

6.4A Transmit signal quality for CA 409

6.4A.1 Frequency error for CA 409

6.4A.1.1 Frequency error for intra-band contiguous CA 409

6.4A.1.2 Frequency error for intra-band non-contiguous CA 410

6.4A.1.3 Frequency error for inter-band CA 410

6.4A.1.4 Void 410

6.4A.2 Transmit modulation quality for CA 410

6.4A.2.1 Transmit modulation quality for intra-band contiguous CA 410

6.4A.2.1.0 General 410

6.4A.2.1.1 Error Vector Magnitude 410

6.4A.2.1.2 In-band emissions 411

6.4A.2.1.3 Carrier leakage 414

6.4A.2.2 Transmit modulation quality for intra-band non-contiguous CA 414

6.4A.2.2.0 General 414

6.4A.2.2.1 Error Vector Magnitude 414

6.4A.2.2.2 In-band emissions 415

6.4A.2.2.3 Carrier leakage 415

6.4A.2.3 Transmit modulation quality for inter-band CA 415

6.4A.2.4 Void 416

6.4B Transmit signal quality for NR-DC 416

6.4C Transmit signal quality for SUL 416

6.4D Transmit signal quality for UL MIMO 416

6.4D.0 General 416

6.4D.1 Frequency error for UL MIMO 416

6.4D.2 Transmit modulation quality for UL MIMO 417

6.4D.2.0 General 417

6.4D.2.1 Error Vector Magnitude 417

6.4D.2.2 Carrier leakage 417

6.4D.2.3 In-band emissions 417

6.4D.2.4 EVM equalizer spectrum flatness for UL MIMO 417

6.4D.3 Time alignment error for UL MIMO 417

6.4D.4 Requirements for coherent UL MIMO 418

6.4E Transmit signal quality for V2X 418

6.4E.1 Frequency error for V2X 418

6.4E.1.1 General 418

6.4E.1.2 Frequency error for V2X con-current operation 419

6.4E.2 Transmit modulation quality for V2X 419

6.4E.2.1 General 419

6.4E.2.2 Error Vector Magnitude for V2X 419

6.4E.2.3 Carrier leakage for V2X 419

6.4E.2.4 In-band emissions for V2X 419

6.4E.2.5 EVM equalizer spectrum flatness for V2X 419

6.4E.2.6 Transmit modulation quality for V2X con-current operation 419

6.4F Transmit signal quality for shared spectrum channel access 420

6.4F.1 Frequency error 420

6.4F.2 Transmit modulation quality 420

6.4F.2.0 General 420

6.4F.2.1 Error Vector Magnitude 420

6.4F.2.2 Carrier leakage 420

6.4F.2.3 In-band emissions 420

6.4F.2.4 EVM equalizer spectrum flatness 421

6.4F.2A Transmit modulation quality for CA 421

6.4F.2A.1 Transmit modulation quality for inter-band CA 421

6.4G Transmit signal quality for Tx Diversity 422

6.4G.1 Frequency error for Tx Diversity 422

6.4G.2 Transmit modulation quality for Tx Diversity 422

6.4G.2.0 General 422

6.4H Transmit signal quality for CA with UL MIMO 423

6.4H.1 Transmit signal quality for intra-band UL contiguous CA with UL MIMO 423

6.4H.1.1 Frequency error for intra-band UL contiguous CA with UL MIMO 423

6.4H.1.2 Transmit modulation quality for intra-band UL contiguous CA with UL MIMO 423

6.4H.1.2.0 General 423

6.4H.1.2.1 Error Vector Magnitude 423

6.4H.1.2.2 Carrier leakage 423

6.4H.1.2.3 In-band emissions 423

6.4H.1.3 Time alignment error for intra-band UL contiguous CA with UL MIMO 423

6.4H.1.4 Coherent UL MIMO requirement for intra-band UL contiguous CA with UL MIMO 424

6.5 Output RF spectrum emissions 424

6.5.1 Occupied bandwidth 424

6.5.2 Out of band emission 424

6.5.2.1 General 424

6.5.2.2 Spectrum emission mask 424

6.5.2.3 Additional spectrum emission mask 425

6.5.2.3.1 Requirements for network signalling value "NS\_35" 425

6.5.2.3.2 Requirements for network signalling value "NS\_04" 425

6.5.2.3.3 Requirements for network signalling values "NS\_03" and “NS\_03U” 426

6.5.2.3.4 Requirements for network signalling value "NS\_06" or “NS\_07” 427

6.5.2.3.5 Void 427

6.5.2.3.6 Void 427

6.5.2.3.7 Void 427

6.5.2.3.8 Requirements for network signalling value "NS\_27" 427

6.5.2.3.9 Requirements for network signalling value "NS\_21" 428

6.5.2.4 Adjacent channel leakage ratio 428

6.5.2.4.1 NR ACLR 428

6.5.2.4.2 UTRA ACLR 429

6.5.3 Spurious emissions 429

6.5.3.0 General 429

6.5.3.1 General spurious emissions 430

6.5.3.2 Spurious emissions for UE co-existence 430

6.5.3.3 Additional spurious emissions 438

6.5.3.3.1 Requirement for network signalling value "NS\_04" 438

6.5.3.3.2 Requirement for network signalling value "NS\_17" 439

6.5.3.3.3 Requirement for network signalling value "NS\_18" 439

6.5.3.3.4 Requirement for network signalling values "NS\_05" and “NS\_05U” 439

6.5.3.3.5 Requirement for network signalling values "NS\_43" and “NS\_43U” 439

6.5.3.3.6 Requirement for network signalling value "NS\_37" 440

6.5.3.3.7 Requirement for network signalling value "NS\_38" 440

6.5.3.3.8 Requirement for network signalling value "NS\_39" 440

6.5.3.3.9 Requirement for network signalling value "NS\_40" 440

6.5.3.3.10 Requirement for network signalling value "NS\_41" 441

6.5.3.3.11 Requirement for network signalling value "NS\_42" 441

6.5.3.3.12 Requirement for network signalling value "NS\_21" 441

6.5.3.3.13 Requirement for network signalling value "NS\_24" 442

6.5.3.3.14 Requirement for network signalling value "NS\_27" 442

6.5.3.3.15 Requirement for network signalling value "NS\_47" 442

6.5.3.3.16 Requirement for network signalling value "NS\_50" 443

6.5.3.3.17 Requirement for network signalling value "NS\_12" 443

6.5.3.3.18 Requirement for network signalling value "NS\_13" 443

6.5.3.3.19 Requirement for network signalling value "NS\_14" 444

6.5.3.3.20 Requirement for network signalling value "NS\_15" 444

6.5.3.3.21 Requirement for network signalling value "NS\_45" 444

6.5.3.3.22 Requirement for network signalling values "NS\_48" and "NS\_51" 445

6.5.3.3.23 Requirement for network signalling value "NS\_49" 445

6.5.3.3.24 Requirement for network signalling value "NS\_44" 445

6.5.3.3.25 Requirement for network signalling value "NS\_46" 446

6.5.3.3.26 Requirement for network signalling value "NS\_07" 446

6.5.3.3.27 Requirement for network signalling value “NS\_56” 446

6.5.4 Transmit intermodulation 447

6.5A Output RF spectrum emissions for CA 447

6.5A.0 General 447

6.5A.1 Occupied bandwidth for CA 448

6.5A.1.1 Void 448

6.5A.1.1a Occupied bandwidth for Intra-band contiguous CA 448

6.5A.1.2 Occupied bandwidth for Intra-band non-contiguous CA 448

6.5A.1.3 Occupied bandwidth for Inter-band CA 448

6.5A.2 Out of band emission for CA 448

6.5A.2.1 General 448

6.5A.2.2 Spectrum emission mask 448

6.5A.2.2.1 Spectrum emission mask for intra-band contiguous CA 448

6.5A.2.2.2 Spectrum emission mask for intra-band non-contiguous CA 449

6.5A.2.2.3 Spectrum emission mask for Inter-band CA 449

6.5.A.2.2.4 Void 449

6.5A.2.3 Additional spectrum emission mask for CA 449

6.5A.2.3.1 Additional spectrum emission mask for intra-band contiguous CA 449

6.5A.2.3.2 Additional spectrum emission mask for Intra-band non-contiguous CA 450

6.5A.2.3.3 Additional spectrum emission mask for Inter-band CA 450

6.5A.2.4 Adjacent channel leakage ratio 450

6.5A.2.4.1 NR ACLR 450

6.5A.2.4.2 UTRA ACLR 452

6.5A.3 Spurious emission for CA 452

6.5A.3.1 General spurious emissions 452

6.5A.3.2 Spurious emissions for UE co-existence 453

6.5A.3.2.1 Spurious emissions for UE co-existence for intra-band contiguous CA 453

6.5A.3.2.2 Spurious emissions for UE co-existence for intra-band non-contiguous CA 455

6.5A.3.2.3 Spurious emissions for UE co-existence for Inter-band CA 455

6.5A.3.2.4 Void 476

6.5A.3.2.5 Void 476

6.5A.3.2.6 Void 476

6.5A.3.3 Additional spurious emissions for CA 476

6.5A.3.3.1 Additional spurious emissions for intra-band contiguous CA 476

6.5A.3.3.2 Additional spurious emissions for intra-band non-contiguous CA 477

6.5A.4 Transmit intermodulation for CA 477

6.5A.4.2.1 Transmit intermodulation for intra-band contiguous CA 477

6.5A.4.2.2 Void 477

6.5B Output RF spectrum emissions for NR-DC 478

6.5D Output RF spectrum emissions for UL MIMO 478

6.5D.1 Occupied bandwidth for UL MIMO 478

6.5D.2 Out of band emission for UL MIMO 478

6.5D.3 Spurious emission for UL MIMO 478

6.5D.4 Transmit intermodulation for UL MIMO 479

6.5E Output RF spectrum emissions for V2X 479

6.5E.1 Occupied bandwidth for V2X 479

6.5E.1.1 General 479

6.5E.1.2 Occupied bandwidth for V2X con-current operation 479

6.5E.2 Out of band emission for V2X 479

6.5E.2.1 General 479

6.5E.2.2 Spectrum emission mask 480

6.5E.2.2.1 General 480

6.5E.2.2.2 Spectrum emission mask for V2X con-current operation 480

6.5E.2.3 Additional Spectrum emission mask 480

6.5E.2.3.1 Requirements for network signalling value "NS\_33" 480

6.5E.2.3.2 Requirements for network signalling value "NS\_52" 480

6.5E.2.3.3 Requirements for network signalling value "NS\_06" 481

6.5E.2.4 Adjacent channel leakage ratio 481

6.5E.2.4.1 General 481

6.5E.2.4.2 ACLR for V2X con-current operation 481

6.5E.3 Spurious emissions for V2X 482

6.5E.3.1 General spurious emissions 482

6.5E.3.2 Spurious emissions for UE co-existence 482

6.5E.3.3 Spurious emissions for UE co-existence for V2X con-current operation 482

6.5E.3.4 Additional spurious emissions requirements for V2X 484

6.5E.3.4.1 General 484

6.5E.3.4.2 Requirements for network signalling value "NS\_33" 484

6.5E.3.4.3 Void 484

6.5E.4 Transmit intermodulation 484

6.5E.4.1 General 484

6.5E.4.2 Transmit intermodulation for V2X con-current operation 484

6.5F Output RF spectrum emissions for shared spectrum channel access 485

6.5F.1 Occupied bandwidth 485

6.5F.2 Out of band emission 485

6.5F.2.1 General 485

6.5F.2.2 Spectrum emission mask for operation with shared spectrum channel access 485

6.5F.2.2.0 General 485

6.5F.2.2.1 Spectrum emission mask for non-transmitted channels 486

6.5F.2.3 Additional spectrum emission mask 486

6.5F.2.4 Adjacent channel leakage ratio 486

6.5F.2.4.0 General 486

6.5F.2.4.1 Shared spectrum channel access ACLR 486

6.5F.2.4.2 Additional requirement for network signalled value "NS\_29" 486

6.5F.2A Out of band emission for CA 487

6.5F.2A.1 Spectrum emission mask for CA 487

6.5F.2A.1.1 Spectrum emission mask for Inter-band CA 487

6.5F.2A.1.2 Spectrum emission mask for Intra-band contiguous CA 487

6.5F.2A.1.2.1 General 487

6.5F.2A.1.2.2 Intra-band contiguous CA spectrum emission mask for non-transmitted channels 487

6.5F.2A.2 Adjacent channel leakage ratio for CA 488

6.5F.2A.2.1 Adjacent channel leakage ratio for inter-band CA 488

6.5F.2A.2.2 Adjacent channel leakage ratio for intra-band contiguous CA 488

6.5F.3 Spurious emissions 488

6.5F.3.0 General 488

6.5F.3.1 General spurious emissions 489

6.5F.3.2 Spurious emissions for UE co-existence 489

6.5F.3.3 Additional spurious emissions 489

6.5F.3.3.0 General 489

6.5F.3.3.1 Requirement for network signalling value "NS\_28" 489

6.5F.3.3.2 Requirement for network signalling value "NS\_29" 489

6.5F.3.3.3 Requirement for network signalling value "NS\_30" 491

6.5F.3.3.4 Requirement for network signalling value "NS\_31" 492

6.5F.3.3.5 Requirements for network signalling value "NS\_53" or "NS\_54" or "NS\_60" 493

6.5F.3.3.6 Requirements for network signalling value "NS\_58" 493

6.5F.3.3.7 Requirements for network signalling value "NS\_61" 493

6.5F.4 Transmit intermodulation 493

6.5G Output RF spectrum emissions for Tx Diversity 494

6.5G.1 Occupied bandwidth for Tx Diversity 494

6.5G.2 Out of band emission for Tx Diversity 494

6.5G.3 Spurious emission for Tx Diversity 494

6.5G.4 Transmit intermodulation for Tx Diversity 494

6.5H Output RF spectrum emissions for CA with UL MIMO 494

6.5H.1 Output RF spectrum emissions for intra-band UL contiguous CA with UL MIMO 494

6.5H.1.1 Occupied bandwidth for intra-band UL contiguous CA with UL MIMO 494

6.5H.1.2 Out of band emission for intra-band UL contiguous CA with UL MIMO 494

6.5H.1.3 Spurious emission for intra-band UL contiguous CA with UL MIMO 495

6.5H.1.4 Transmit intermodulation for intra-band UL contiguous CA with UL MIMO 495

6.6 Void 495

6.6E Time alignment error 495

7 Receiver characteristics 496

7.1 General 496

7.1A General 496

7.1F General 497

7.1I General 497

7.2 Diversity characteristics 497

7.3 Reference sensitivity 497

7.3.1 General 497

7.3.2 Reference sensitivity power level 497

7.3.3 ΔRIB,c 508

7.3A Reference sensitivity for CA 508

7.3A.1 General 508

7.3A.2 Reference sensitivity power level for CA 508

7.3A.2.1 Reference sensitivity power level for Intra-band contiguous CA 508

7.3A.2.2 Reference sensitivity power level for Intra-band non-contiguous CA 509

7.3A.2.3 Reference sensitivity power level for Inter-band CA 510

7.3A.2.4 Void 510

7.3A.3 ΔRIB,c for CA 511

7.3A.3.1 General 511

7.3A.3.2 ΔRIB,c for Inter-band CA 511

7.3A.3.2.1 ΔRIB,c for two bands 512

7.3A.3.2.2 Void 516

7.3A.3.2.3 ΔRIB,c for three bands 516

7.3A.3.2.4 ΔRIB,c for four bands 525

7.3A.3.2.5 ΔRIB,c for five bands 531

7.3A.3.3 ΔRIB,c for Intra-band CA 531

7.3A.4 Reference sensitivity exceptions due to UL harmonic interference for CA 531

7.3A.5 Reference sensitivity exceptions due to intermodulation interference due to 2UL CA 540

7.3A.6 Reference sensitivity exceptions due to cross band isolation for CA 567

7.3B Reference sensitivity for NR-DC 571

7.3C Reference sensitivity for SUL 571

7.3C.1 General 571

7.3C.2 Reference sensitivity power level for SUL 571

7.3C.3 ΔRIB,c for SUL 575

7.3C.3.1 General 575

7.3C.3.2 SUL band combination 575

7.3C.3.2.1 ΔRIB,c for two bands 575

7.3C.3.2.2 ΔRIB,c for three bands 576

7.3C.3.2.3 ΔRIB,c for four bands 576

7.3D Reference sensitivity for UL MIMO 576

7.3E Reference sensitivity for V2X 577

7.3E.1 General 577

7.3E.2 Minimum requirements 577

7.3E.3 Reference sensitivity power level for V2X con-current operation 578

7.3F Reference sensitivity for shared spectrum channel access 579

7.3F.1 General 579

7.3F.2 Reference sensitivity power level 580

7.3F.3 Void 580

7.3F.4 Void 581

7.3F.4A Shared spectrum channel access CA 581

7.3F.4A.1 Intra-band contiguous shared spectrum channel access CA 581

7.3F.5 Void 581

7.3F.5.1 Void 581

7.3F.5.2 Void 581

7.3F.5.3 Void 581

7.3G Reference sensitivity for Tx Diversity 581

7.3G.5 Void 581

7.3G.5.0 Void 581

7.3I Reference sensitivity for RedCap 581

7.3I.1 General 581

7.3I.2 Reference sensitivity power level 581

7.4 Maximum input level 589

7.4A Maximum input level for CA 589

7.4A.1 Maximum input level for Intra-band contiguous CA 589

7.4A.2 Maximum input level for Intra-band non-contiguous CA 590

7.4A.3 Maximum input level for Inter-band CA 590

7.4B Maximum input level for NR-DC 590

7.4D Maximum input level for UL MIMO 590

7.4E Maximum input level for V2X 590

7.4E.1 General 590

7.4E.2 Maximum input level for V2X con-current operation 591

7.5 Adjacent channel selectivity 591

7.5A Adjacent channel selectivity for CA 593

7.5A.1 Adjacent channel selectivity for Intra-band contiguous CA 593

7.5A.2 Adjacent channel selectivity Intra-band non-contiguous CA 595

7.5A.3 Adjacent channel selectivity Inter-band CA 596

7.5B Adjacent channel selectivity for NR-DC 596

7.5D Adjacent channel selectivity for UL MIMO 596

7.5E Adjacent channel selectivity for V2X 596

7.5E.1 General 596

7.5E.2 Adjacent channel selectivity for V2X con-current operation 598

7.5F Adjacent channel selectivity for shared spectrum channel access 598

7.5F.1 General 598

7.5F.1A Adjacent channel selectivity for shared spectrum channel access CA 599

7.5F.1A.1 Intra-band contiguous shared spectrum channel access CA 599

7.5F.2 Void 600

7.6 Blocking characteristics 600

7.6.1 General 600

7.6.2 In-band blocking 600

7.6.3 Out-of-band blocking 602

7.6.4 Narrow band blocking 605

7.6A Blocking characteristics for CA 606

7.6A.1 General 606

7.6A.2 In-band blocking for CA 606

7.6A.2.1 In-band blocking for Intra-band contiguous CA 606

7.6A.2.2 In-band blocking for Intra-band non-contiguous CA 608

7.6A.2.3 In-band blocking for Inter-band CA 608

7.6A.3 Out-of-band blocking for CA 609

7.6A.3.1 Out-of-band blocking for Intra-band contiguous CA 609

7.6A.3.2 Out-of-band blocking for Intra-band non-contiguous CA 610

7.6A.3.3 Out-of-band blocking for Inter-band CA 610

7.6A.4 Narrow band blocking for CA 612

7.6A.4.1 Narrow band blocking for Intra-band contiguous CA 612

7.6A.4.2 Narrow band blocking for Intra-band non-contiguous CA 612

7.6A.4.3 Narrow band blocking for Inter-band CA 612

7.6B Blocking characteristics for NR-DC 613

7.6C Blocking characteristics for SUL 613

7.6C.1 General 613

7.6C.2 In-band blocking for SUL 613

7.6C.3 Out-of-band blocking for SUL 613

7.6C.4 Narrow band blocking for SUL 614

7.6D Blocking characteristics for UL MIMO 614

7.6E Blocking characteristics for V2X 614

7.6E.1 General 614

7.6E.2 In-band blocking 614

7.6E.2.1 General 614

7.6E.2.2 In-band blocking for V2X con-current operation 615

7.6E.3 Out-of-band blocking 615

7.6E.3.1 General 615

7.6E.3.2 Out-of-band blocking for V2X con-current operation 616

7.6F Blocking characteristics for shared spectrum channel access 616

7.6F.1 General 616

7.6F.2 In-band blocking 616

7.6F.2.1 General 616

7.6F.2.2 Void 617

7.6F.2A In-band blocking for shared spectrum CA 617

7.6F.2A.1 Intra-band contiguous shared spectrum channel access CA 617

7.6F.3 Out-of-band blocking 618

7.6F.3.1 General 618

7.6F.3.2 Void 619

7.6F.3A Out-of-band blocking for shared spectrum CA 619

7.6F.3A.1 Intra-band contiguous shared spectrum channel access CA 619

7.7 Spurious response 620

7.7A Spurious response for CA 621

7.7A.1 Spurious response for Intra-band contiguous CA 621

7.7A.2 Spurious response for Intra-band non-contiguous CA 621

7.7A.3 Spurious response for Inter-band CA 621

7.7B Spurious response for NR-DC 622

7.7D Spurious response for UL MIMO 622

7.7E Spurious response for V2X 622

7.7E.1 General 622

7.7E.2 Spurious response for V2X con-current operation 622

7.7F Spurious response for shared spectrum channel access 622

7.7F.1 General 622

7.7F.1A Spurious response for shared spectrum channel access CA 623

7.7F.1A.1 Intra-band contiguous shared spectrum channel access CA 623

7.7F.2 Void 623

7.8 Intermodulation characteristics 624

7.8.1 General 624

7.8.2 Wide band Intermodulation 624

7.8A Intermodulation characteristics for CA 626

7.8A.1 General 626

7.8A.2 Wide band intermodulation for CA 626

7.8A.2.1 Wide band intermodulation for Intra-band contiguous CA 626

7.8A.2.2 Wide band intermodulation for Intra-band non-contiguous CA 627

7.8A.2.3 Wide band intermodulation for Inter-band CA 627

7.8B Intermodulation characteristics for NR-DC 627

7.8D Intermodulation characteristics for UL MIMO 628

7.8E Intermodulation characteristics for V2X 628

7.8E.1 General 628

7.8E.2 Wide band Intermodulation 628

7.8E.2.1 General 628

7.8E.2.2 Wide band Intermodulation for V2X con-current operation 629

7.8F Intermodulation characteristics for shared spectrum channel access 629

7.8F.1 General 629

7.8F.2 Wide band Intermodulation 629

7.9 Spurious emissions 630

7.9A Spurious emissions for CA 630

7.9A.1 Void 630

7.9A.2 Void 630

7.9A.3 Spurious emissions for Inter-band CA 630

7.9B Spurious emissions for NR-DC 631

Annex A (normative): Measurement channels 626

A.1 General 626

A.2 UL reference measurement channels 626

A.2.1 General 626

A.2.2 Reference measurement channels 628

A.2.2.1 DFT-s-OFDM Pi/2-BPSK 628

A.2.2.2 DFT-s-OFDM QPSK 629

A.2.2.3 DFT-s-OFDM 16QAM 629

A.2.2.4 DFT-s-OFDM 64QAM 631

A.2.2.5 DFT-s-OFDM 256QAM 633

A.2.2.6 CP-OFDM QPSK 635

A.2.2.7 CP-OFDM 16QAM 637

A.2.2.8 CP-OFDM 64QAM 639

A.2.2.9 CP-OFDM 256QAM 641

A.2.3 Reference measurement channels for TDD 643

A.2.3.1 DFT-s-OFDM Pi/2-BPSK 643

A.2.3.2 DFT-s-OFDM QPSK 643

A.2.3.3 DFT-s-OFDM 16QAM 643

A.2.3.4 DFT-s-OFDM 64QAM 643

A.2.3.5 DFT-s-OFDM 256QAM 644

A.2.3.6 CP-OFDM QPSK 644

A.2.3.7 CP-OFDM 16QAM 644

A.2.3.8 CP-OFDM 64QAM 644

A.2.3.9 CP-OFDM 256QAM 645

A.3 DL reference measurement channels 646

A.3.1 General 646

A.3.2 DL reference measurement channels for FDD 647

A.3.2.1 General 647

A.3.2.2 FRC for receiver requirements for QPSK 647

A.3.2.3 FRC for maximum input level for 64QAM 650

A.3.2.4 FRC for maximum input level for 256 QAM 653

A.3.2.5 FRC for maximum input level for 1024 QAM 656

A.3.3 DL reference measurement channels for TDD 659

A.3.3.1 General 659

A.3.3.2 FRC for receiver requirements for QPSK 660

A.3.3.3 FRC for maximum input level for 64QAM 663

A.3.3.4 FRC for maximum input level for 256 QAM 666

A.3.3.5 FRC for maximum input level for 1024 QAM 669

A.4 CSI reference measurement channels 672

A.5 OFDMA Channel Noise Generator (OCNG) 672

A.5.1 OCNG Patterns for FDD 672

A.5.1.1 OCNG FDD pattern 1: Generic OCNG FDD Pattern for all unused REs 672

A.5.2 OCNG Patterns for TDD 672

A.5.2.1 OCNG TDD pattern 1: Generic OCNG TDD Pattern for all unused REs 672

A.6 Void 673

A.7 V2X reference measurement channels 673

A.7.1 General 673

A.7.2 FRC for V2X receiver requirements for QPSK 673

A.7.3 FRC for maximum input level for 64QAM 675

A.7.4 FRC for maximum input level for 256QAM 676

Annex B (informative): Void 678

Annex C (informative): Downlink physical channels 679

C.1 General 679

C.2 Setup 679

C.3 Connection 679

C.3.1 Measurement of Receiver Characteristics 679

Annex D (normative): Characteristics of the interfering signal 681

D.1 General 681

D.2 Interference signals 681

Annex E (normative): Environmental conditions 682

E.1 General 682

E.2 Environmental 682

E.2.1 Temperature 682

E.2.2 Voltage 683

E.2.3 Vibration 683

Annex F (normative): Transmit modulation 684

F.0 General 684

F.1 Measurement Point 684

F.2 Basic Error Vector Magnitude measurement 684

F.3 Basic in-band emissions measurement 685

F.4 Modified signal under test 685

F.5 Window length 688

F.5.1 Timing offset 688

F.5.2 Window length 688

F.5.3 Window length for normal CP 688

F.5.4 Window length for Extended CP 689

F.5.5 Window length for PRACH 690

F.6 Averaged EVM 691

F.7 Spectrum Flatness 692

F.8 EVM measurement for dual Tx 692

F.9 Phase offset measurement for DMRS bundling 692

F.9.1 Measurement point 692

F.9.2 Symbols used 692

F.9.3 Modified test signal 692

F.9.4 Phase offset measurement 693

F.10 EVM for UL MIMO 693

F10.1 General 693

F10.2 MIMO Equalization 694

F10.3 Layer processing 694

Annex G (normative): Difference of relative phase and power errors 696

G.0 General 696

G.1 Measurement Point 696

G.2 Relative Phase Error Measurement 696

G.2.1 Symbols and subcarriers used 696

G.2.2 CFO (carrier frequency offset) correction 697

G.2.3 Steps of the measurement method 697

Annex H (informative): Void 698

Annex I (informative): Void 698

Annex J (informative): Void 698

Annex K (informative): Void 698

Annex L (normative): ModifiedMPR-Behavior 698

L.1 Indication of modified MPR behavior 698

Annex M (informative): Change history 702