|  |  |
| --- | --- |
| 3GPP TS 36.101 V17.8.0 (2022-12) | |
| Technical Specification | |
| 3rd Generation Partnership Project;  Technical Specification Group Radio Access Network;  Evolved Universal Terrestrial Radio Access (E-UTRA);  User Equipment (UE) radio transmission and reception  (Release 17) | |
|  | |
| *LTE-AdvancedPro_largerTM_cropped* | 3GPP-logo_web |
|  | |
| The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP. The present document has not been subject to any approval process by the 3GPPOrganizational Partners and shall not be implemented. This Specification is provided for future development work within 3GPPonly. The Organizational Partners accept no liability for any use of this Specification. Specifications and Reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organizational Partners' Publications Offices. | |

|  |
| --- |
|  |
| ***3GPP***  Postal address  3GPP support office address  650 Route des Lucioles - Sophia Antipolis  Valbonne - FRANCE  Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16  Internet  http://www.3gpp.org |
| ***Copyright Notification***  No part may be reproduced except as authorized by written permission. The copyright and the foregoing restriction extend to reproduction in all media.  © 2022, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).  All rights reserved.  UMTS™ is a Trade Mark of ETSI registered for the benefit of its members  3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  GSM® and the GSM logo are registered and owned by the GSM Association |

Contents

Foreword 32

1 Scope 34

2 References 34

3 Definitions, symbols and abbreviations 34

3.1 Definitions 34

3.2 Symbols 36

3.3 Abbreviations 39

4 General 41

4.1 Relationship between minimum requirements and test requirements 41

4.2 Applicability of minimum requirements 41

4.3 Void 41

4.3A Applicability of minimum requirements (CA, UL-MIMO, ProSe, Dual Connectivity, UE category 0, UE category M1, UE category M2, UE category 1bis, UE category NB1 and NB2, V2X Communication, MBMS UE) 41

4.4 RF requirements in later releases 43

5 Operating bands and channel arrangement 43

5.1 General 43

5.2 Void 43

5.3 Void 43

5.4 Void 43

5.5 Operating bands 43

5.5A Operating bands for CA 46

5.5B Operating bands for UL-MIMO 67

5.5C Operating bands for Dual Connectivity 67

5.5D Operating bands for ProSe 70

5.5E Operating bands for UE category 0, UE category M1 and M2 and UE category 1bis 71

5.5F Operating bands for category NB1 and NB2 71

5.5G Operating bands for V2X Communication 72

5.6 Channel bandwidth 73

5.6.1 Channel bandwidths per operating band 74

5.6A Channel bandwidth for CA 77

5.6A.1 Channel bandwidths per operating band for CA 79

5.6B Channel bandwidth for UL-MIMO 203

5.6B.1 Void 203

5.6C Channel bandwidth for Dual Connectivity 203

5.6C.1 Void 203

5.6D Channel bandwidth for ProSe 203

5.6D.1 Channel bandwidths per operating band for ProSe 203

5.6F Channel bandwidth for category NB1 and NB2 204

5.6G Channel bandwidth for V2X Communication 205

5.6G.1 Channel bandwidths per operating band for V2X Communication 205

5.7 Channel arrangement 207

5.7.1 Channel spacing 207

5.7.1A Channel spacing for CA 207

5.7.1F Channel spacing for category NB1 and NB2 208

5.7.2 Channel raster 208

5.7.2A Channel raster for CA 208

5.7.2F Channel raster for category NB1 and NB2 208

5.7.3 Carrier frequency and EARFCN 208

5.7.3F Carrier frequency and EARFCN for category NB1 and NB2 211

5.7.4 TX–RX frequency separation 212

5.7.4A TX–RX frequency separation for CA 212

5.7.4E TX–RX frequency separation for category M1 and M2 213

5.7.4F TX–RX frequency separation for category NB1 and NB2 213

6 Transmitter characteristics 213

6.1 General 213

6.2 Transmit power 213

6.2.1 Void 213

6.2.2 UE maximum output power 213

6.2.2A UE maximum output power for CA 216

6.2.2B UE maximum output power for UL-MIMO 221

6.2.2C Void 224

6.2.2D UE maximum output power for ProSe 224

6.2.2E UE maximum output power for Category M1 and M2 UE 224

6.2.2F UE maximum output power for category NB1 and NB2 225

6.2.2G UE maximum output power for V2X Communication 226

6.2.3 UE maximum output power for modulation / channel bandwidth 228

6.2.3A UE Maximum Output power for modulation / channel bandwidth for CA 229

6.2.3B UE maximum output power for modulation / channel bandwidth for UL-MIMO 234

6.2.3D UE maximum output power for modulation / channel bandwidth for ProSe 234

6.2.3E UE maximum output power for modulation / channel bandwidth for category M1 and M2 235

6.2.3F UE maximum output power for modulation / channel bandwidth for category NB1 and NB2 237

6.2.3G UE maximum output power for modulation / channel bandwidth for V2X Communication 237

6.2.3G.1 MPR for Power class 3 V2X UE 237

6.2.3G.2 MPR for Power class 2 V2X UE 239

6.2.4 UE maximum output power with additional requirements 239

6.2.4A UE maximum output power with additional requirements for CA 258

6.2.4A.1 A-MPR for CA\_NS\_01 for CA\_1C 260

6.2.4A.2 A-MPR for CA\_NS\_02 for CA\_1C 261

6.2.4A.3 A-MPR for CA\_NS\_03 for CA\_1C 261

6.2.4A.4 A-MPR for CA\_NS\_04 262

6.2.4A.5 A-MPR for CA\_NS\_05 for CA\_38C 265

6.2.4A.6 A-MPR for CA\_NS\_06 266

6.2.4A.7 A-MPR for CA\_NS\_07 267

6.2.4A.8 A-MPR for CA\_NS\_08 268

6.2.4A.9 Void 269

6.2.4A.10 A-MPR for CA\_NS\_10 269

6.2.4B UE maximum output power with additional requirements for UL-MIMO 274

6.2.4D UE maximum output power with additional requirements for ProSe 274

6.2.4E UE maximum output power with additional requirements for category M1 and M2 UE 274

6.2.4F UE maximum output power with additional requirements for category NB1 and NB2 UE 285

6.2.4G UE maximum output power with additional requirements for V2X Communication 285

6.2.5 Configured transmitted power 288

6.2.5A Configured transmitted power for CA 323

6.2.5B Configured transmitted power for UL-MIMO 327

6.2.5C Configured transmitted power for Dual Connectivity 327

6.2.5D Configured transmitted power for ProSe 329

6.2.5F Configured transmitted Power for category NB1 and NB2 330

6.2.5G Configured transmitted power for V2X Communication 331

6.3 Output power dynamics 335

6.3.1 (Void) 335

6.3.2 Minimum output power 335

6.3.2.1 Minimum requirement 335

6.3.2A UE Minimum output power for CA 335

6.3.2A.1 Minimum requirement for CA 336

6.3.2B UE Minimum output power for UL-MIMO 336

6.3.2B.1 Minimum requirement 336

6.3.2C Void 336

6.3.2D UE Minimum output power for ProSe 336

6.3.2F UE Minimum output power for category NB1 and NB2 337

6.3.2G UE Minimum output power for V2X Communication 337

6.3.3 Transmit OFF power 337

6.3.3.1. Minimum requirement 337

6.3.3A UE Transmit OFF power for CA 338

6.3.3A.1 Minimum requirement for CA 338

6.3.3B UE Transmit OFF power for UL-MIMO 338

6.3.3B.1 Minimum requirement 338

6.3.3D Transmit OFF power for ProSe 339

6.3.3F Transmit OFF power for category NB1 and NB2 339

6.3.3G Transmit OFF power for V2X Communication 339

6.3.4 ON/OFF time mask 340

6.3.4.1 General ON/OFF time mask 340

6.3.4.2 PRACH and SRS time mask 341

6.3.4.2.1 PRACH time mask 341

6.3.4.2.2 SRS time mask 342

6.3.4.3 Slot / Sub frame boundary time mask for subframe TTI 344

6.3.4.4 PUCCH / PUSCH / SRS time mask for subframe TTI 346

6.3.4.5 Symbol / Subslot boundary time mask for subslot TTI 348

6.3.4.6 Subslot PUCCH / subslot PUSCH / SRS time mask for subslot TTI 349

6.3.4.7 Symbol / Slot boundary time mask for slot TTI 352

6.3.4.8 Slot PUCCH / slot PUSCH / SRS time mask for slot TTI 353

6.3.4.9 Consecutive subslot and slot TTI or consecutive subslot and subframe TTI time mask 353

6.3.4.10 Consecutive subframe and subslot TTI or consecutive slot and subslot TTI time mask 353

6.3.4.11 Consecutive TTI and slot TTI or consecutive slot TTI and TTI time mask 354

6.3.4A ON/OFF time mask for CA 355

6.3.4B ON/OFF time mask for UL-MIMO 355

6.3.4D ON/OFF time mask for ProSe 355

6.3.4D.1 General time mask for ProSe 355

6.3.4D.2 PSSS/SSSS time mask 356

6.3.4D.3 PSSS / SSSS / PSBCH time mask 357

6.3.4D.4 PSSCH / SRS time mask 357

6.3.4F ON/OFF time mask for category NB1 and NB2 357

6.3.4F.1 General ON/OFF time mask 357

6.3.4F.2 NPRACH time mask 358

6.3.4G ON/OFF time mask for V2X Communication 358

6.3.4G.1 PSSS / SSSS / PSBCH time mask 359

6.3.5 Power Control 359

6.3.5.1 Absolute power tolerance 359

6.3.5.1.1 Minimum requirements 359

6.3.5.2 Relative Power tolerance 360

6.3.5.2.1 Minimum requirements 360

6.3.5.3 Aggregate power control tolerance 361

6.3.5.3.1 Minimum requirement 361

6.3.5A Power control for CA 361

6.3.5A.1 Absolute power tolerance 361

6.3.5A.1.1 Minimum requirements 361

6.3.5A.2 Relative power tolerance 362

6.3.5A.2.1 Minimum requirements 362

6.3.5A.3 Aggregate power control tolerance 362

6.3.5A.3.1 Minimum requirements 362

6.3.5B Power control for UL-MIMO 363

6.3.5D Power Control for ProSe 363

6.3.5D.1 Absolute power tolerance 363

6.3.5E Power control for category M1 and M2 363

6.3.5E.1 Absolute power tolerance 363

6.3.5E.2 Relative Power tolerance 363

6.3.5E.3 Aggregate power control tolerance 364

6.3.5E.3.1 Minimum requirement 364

6.3.5F Power Control for category NB1 and NB2 364

6.3.5F.1 Absolute power tolerance 365

6.3.5F.2 Relative power tolerance 365

6.3.5F.3 Aggregate power control tolerance for category NB1 and NB2 366

6.3.5F.3.1 Minimum requirement 366

6.3.5G Power Control for V2X Communication 366

6.3.5G.1 Absolute power tolerance 366

6.4 Void 367

6.5 Transmit signal quality 367

6.5.1 Frequency error 367

6.5.1A Frequency error for CA 367

6.5.1B Frequency error for UL-MIMO 367

6.5.1D Frequency error for ProSe 367

6.5.1E Frequency error for UE category M1 and M2 367

6.5.1F Frequency error for UE category NB1 and NB2 368

6.5.1G Frequency error for V2X Communication 368

6.5.2 Transmit modulation quality 368

6.5.2.1 Error Vector Magnitude 369

6.5.2.1.1 Minimum requirement 369

6.5.2.2 Carrier leakage 369

6.5.2.2.1 Minimum requirements 370

6.5.2.3 In-band emissions 370

6.5.2.3.1 Minimum requirements 370

6.5.2.4 EVM equalizer spectrum flatness 371

6.5.2.4.1 Minimum requirements 371

6.5.2A Transmit modulation quality for CA 372

6.5.2A.1 Error Vector Magnitude 373

6.5.2A.2 Carrier leakage for CA 373

6.5.2A.2.1 Minimum requirements 373

6.5.2A.3 In-band emissions 373

6.5.2A.3.1 Minimum requirement for CA 373

6.5.2B Transmit modulation quality for UL-MIMO 376

6.5.2B.1 Error Vector Magnitude 376

6.5.2B.2 Carrier leakage 376

6.5.2B.3 In-band emissions 376

6.5.2B.4 EVM equalizer spectrum flatness for UL-MIMO 376

6.5.2D Transmit modulation quality for ProSe 376

6.5.2D.1 Error Vector Magnitude 376

6.5.2D.2 Carrier leakage 377

6.5.2D.3 In-band emissions 377

6.5.2D.4 EVM equalizer spectrum flatness for ProSe 377

6.5.2E Transmit modulation quality for category M1 and M2 377

6.5.2E.1 Error Vector Magnitude 377

The Error Vector Magnitude is defined in section 6.5.2.1. 377

6.5.2E.2 Carrier leakage 377

6.5.2E.2.1 Minimum requirements 377

6.5.2E.3 In-band emissions 377

6.5.2E.3.1 Minimum requirements 377

6.5.2F Transmit modulation quality for Category NB1 and NB2 379

6.5.2F.1 Error Vector Magnitude 379

6.5.2F.2 Carrier leakage 379

6.5.2F.3 In-band emissions 379

6.5.2G Transmit modulation quality for V2X Communication 380

6.5.2G.1 Error Vector Magnitude 380

6.5.2G.2 Carrier leakage 381

6.5.2G.3 In-band emissions 381

6.5.2G.4 EVM equalizer spectrum flatness 381

6.6 Output RF spectrum emissions 381

6.6.1 Occupied bandwidth 381

6.6.1.1 Additional minimum requirement for E-UTRA (network signalled value “NS\_29”) 382

6.6.1A Occupied bandwidth for CA 382

6.6.1B Occupied bandwidth for UL-MIMO 382

6.6.1F Occupied bandwidth for category NB1 and NB2 383

6.6.1G Occupied bandwidth for V2X Communication 383

6.6.2 Out of band emission 383

6.6.2.1 Spectrum emission mask 383

6.6.2.1.1 Minimum requirement 383

6.6.2.1A Spectrum emission mask for CA 384

6.6.2.2 Additional spectrum emission mask 385

6.6.2.2.1 Minimum requirement (network signalled value "NS\_03", “NS\_11”, "NS\_20", and “NS\_21”) 385

6.6.2.2.2 Minimum requirement (network signalled value "NS\_04") 386

6.6.2.2.3 Minimum requirement (network signalled value "NS\_06" or “NS\_07”) 386

6.6.2.2.4 Minimum requirement (network signalled value "NS\_33" or “NS\_34”) 387

6.6.2.2.5 Minimum requirement (network signalled value “NS\_27” and “NS\_43”) 387

6.6.2.2.6 Minimum requirement (network signalled value "NS\_28”) 388

6.6.2.2.7 Minimum requirement (network signalled value "NS\_35") 388

6.6.2.2A Additional Spectrum Emission Mask for CA 389

6.6.2.2A.1 Minimum requirement (network signalled value "CA\_NS\_04") 389

6.6.2.2A.2 Minimum requirement CA\_66B (network signalled value "CA\_NS\_09") 389

6.6.2.2A.3 Minimum requirement CA\_66C (network signalled value "CA\_NS\_09") 390

6.6.2.2A.4 Minimum requirement CA\_48B and CA\_48C (network signalled value "CA\_NS\_10") 390

6.6.2.3 Adjacent Channel Leakage Ratio 391

6.6.2.3.1 Minimum requirement E-UTRA 391

6.6.2.3.1a Additional minimum requirement for E-UTRA (network signalled value “NS\_29”) 392

6.6.2.3.1A Void 393

6.6.2.3.1Aa Void 393

6.6.2.3.2 Minimum requirements UTRA 393

6.6.2.3.2A Minimum requirement UTRA for CA 394

6.6.2.3.3A Minimum requirements for CA E-UTRA 396

6.6.2.4 Void 397

6.6.2.4.1 Void 397

6.6.2A Void 397

6.6.2B Out of band emission for UL-MIMO 397

6.6.2C Void 397

6.6.2D Out of band emission for ProSe 397

6.6.2F Out of band emission for category NB1 and NB2 398

6.6.2F.1 Spectrum emission mask 398

6.6.2F.2 Additional Spectrum Emission Mask for Category NB1 and NB2 398

6.6.2F.2.1 Minimum requirement (network signalled value "NS\_02") 398

6.6.2F.2.2 Minimum requirement (network signalled value "NS\_03") 398

6.6.2F.3 Adjacent Channel Leakage Ratio for category NB1 and NB2 399

6.6.2G Out of band emission for V2X Communication 399

6.6.3 Spurious emissions 400

6.6.3.1 Minimum requirements 400

6.6.3.1A Minimum requirements for CA 401

6.6.3.2 Spurious emission band UE co-existence 402

6.6.3.2A Spurious emission band UE co-existence for CA 411

6.6.3.3 Additional spurious emissions 427

6.6.3.3.1 Minimum requirement (network signalled value "NS\_05") 428

6.6.3.3.2 Minimum requirement (network signalled value “NS\_07”) 428

6.6.3.3.3 Minimum requirement (network signalled value “NS\_08”) 428

6.6.3.3.4 Minimum requirement (network signalled value “NS\_09”) 428

6.6.3.3.5 Minimum requirement (network signalled value "NS\_12") 429

6.6.3.3.6 Minimum requirement (network signalled value “NS\_13”) 429

6.6.3.3.7 Minimum requirement (network signalled value “NS\_14”) 429

6.6.3.3.8 Minimum requirement (network signalled value “NS\_15”) 430

6.6.3.3.9 Minimum requirement (network signalled value “NS\_16”) 430

6.6.3.3.10 Minimum requirement (network signalled value “NS\_17”) 430

6.6.3.3.11 Minimum requirement (network signalled value “NS\_18”) 430

6.6.3.3.12 Minimum requirement (network signalled value “NS\_19”) 431

6.6.3.3.13 Minimum requirement (network signalled value “NS\_11”) 431

6.6.3.3.14 Minimum requirement (network signalled value “NS\_20”) 431

6.6.3.3.15 Minimum requirement (network signalled value “NS\_21”) 431

6.6.3.3.16 Minimum requirement (network signalled value "NS\_22") 432

6.6.3.3.17 Minimum requirement (network signalled value “NS\_23”) 432

6.6.3.3.18 Void 433

6.6.3.3.19 Minimum requirement (network signalled value "NS\_04") 433

6.6.3.3.20 Minimum requirement (network signalled value “NS\_24”) 433

6.6.3.3.21 Minimum requirement (network signalled value “NS\_25”) 434

6.6.3.3.22 Minimum requirement (network signalled value “NS\_26”) 434

6.6.3.3.23 Minimum requirement (network signalled value “NS\_27” and “NS\_43”) 434

6.6.3.3.24 Minimum requirement (network signalled value “NS\_28”) 434

6.6.3.3.25 Minimum requirement (network signalled value “NS\_29”) 435

6.6.3.3.26 Minimum requirement (network signalled value “NS\_30”) 435

6.6.3.3.27 Minimum requirement (network signalled value “NS\_31”) 436

6.6.3.3.28 Minimum requirement (network signalled value “NS\_36”) 437

6.6.3.3.29 Minimum requirement (network signalled value “NS\_38”) 437

6.6.3.3.30 Minimum requirement (network signalled value “NS\_39”) 437

6.6.3.3.31 Minimum requirement (network signalled value “NS\_40” and “NS\_41”) 438

6.6.3.3.32 Minimum requirement (network signalled value “NS\_42”) 438

6.6.3.3.33 Minimum requirement (network signalled value “NS\_44”) 438

6.6.3.3.34 Minimum requirement (network signalled value “NS\_45”) 438

6.6.3.3.35 Minimum requirement (network signalled value “NS\_56”) 439

6.6.3.3A Additional spurious emissions for CA 439

6.6.3.3A.1 Minimum requirement for CA\_1C (network signalled value "CA\_NS\_01") 440

6.6.3.3A.2 Minimum requirement for CA\_1C (network signalled value "CA\_NS\_02") 440

6.6.3.3A.3 Minimum requirement for CA\_1C (network signalled value "CA\_NS\_03") 440

6.6.3.3A.4 Minimum requirement for CA\_38C (network signalled value "CA\_NS\_05") 441

6.6.3.3A.5 Minimum requirement for CA\_7C (network signalled value "CA\_NS\_06") 441

6.6.3.3A.6 Minimum requirement for CA\_39C and CA\_39C-41A (network signalled value "CA\_NS\_07") 441

6.6.3.3A.7 Minimum requirement for CA\_42C (network signalled value "CA\_NS\_08") 441

6.6.3.3A.8 Minimum requirement for CA\_41C and CA\_41D (network signalled value "CA\_NS\_04") 442

6.6.3.3A.9 Void 442

6.6.3.3A.10 Minimum requirement for CA\_48B and CA\_48C (network signalled value "CA\_NS\_10") 442

6.6.3A Void 442

6.6.3B Spurious emission for UL-MIMO 443

6.6.3C Void 443

6.6.3D Spurious emission for ProSe 443

6.6.3F Spurious emission for category NB1 and NB2 443

6.6.3G Spurious emission for V2X Communication 443

6.6A Void 447

6.6B Void 447

6.7 Transmit intermodulation 447

6.7.1 Minimum requirement 447

6.7.1A Minimum requirement for CA 448

6.7.1B Minimum requirement for UL-MIMO 448

6.7.1F Minimum requirement for category NB1 and NB2 448

6.7.1G Minimum requirement for V2X Communication 449

6.8 Void 449

6.8A Void 449

6.8B Time alignment error for UL-MIMO 449

6.8B.1 Minimum Requirements 449

6.8C Void 450

6.8D Void 450

6.8E Void 450

6.8F Void 450

6.8G Time alignment error 450

7 Receiver characteristics 450

7.1 General 450

7.2 Diversity characteristics 451

7.3 Reference sensitivity power level 451

7.3.1 Minimum requirements (QPSK) 451

7.3.1A Minimum requirements (QPSK) for CA 491

7.3.1B Minimum requirements (QPSK) for UL-MIMO 538

7.3.1D Minimum requirements (QPSK) for ProSe 538

7.3.1E Minimum requirements (QPSK) for UE category 0, M1, M2 and 1bis 540

7.3.1F Minimum requirements for UE category NB1 and NB2 550

7.3.1F.1 Reference sensitivity for UE category NB1 and NB2 550

7.3.1F.2 Void 551

7.3.1G Minimum requirements (QPSK) for V2X 551

7.3.2 Void 553

7.4 Maximum input level 553

7.4.1 Minimum requirements 554

7.4.1A Minimum requirements for CA 554

7.4.1B Minimum requirements for UL-MIMO 555

7.4.1D Minimum requirements for ProSe 555

7.4.1F Minimum requirements for category NB1 and NB2 556

7.4.1G Minimum requirements for V2X 556

7.4A Void 557

7.4A.1 Void 557

7.5 Adjacent Channel Selectivity (ACS) 557

7.5.1 Minimum requirements 557

7.5.1A Minimum requirements for CA 558

7.5.1B Minimum requirements for UL-MIMO 562

7.5.1D Minimum requirements for ProSe 562

7.5.1F Minimum requirements for category NB1 and NB2 563

7.5.1G Minimum requirements for V2X 564

7.6 Blocking characteristics 566

7.6.1 In-band blocking 566

7.6.1.1 Minimum requirements 566

7.6.1.1A Minimum requirements for CA 568

7.6.1.1D Minimum requirements for ProSe 571

7.6.1.1F Minimum requirements for category NB1 and NB2 572

7.6.1.1G Minimum requirements for V2X 572

7.6.2 Out-of-band blocking 574

7.6.2.1 Minimum requirements 574

7.6.2.1A Minimum requirements for CA 576

7.6.2.1D Minimum requirements for ProSe 579

7.6.2.1F Minimum requirements for category NB1 and NB2 579

7.6.2.1G Minimum requirements for V2X 580

7.6.3 Narrow band blocking 581

7.6.3.1 Minimum requirements 581

7.6.3.1A Minimum requirements for CA 582

7.6.3.1D Minimum requirements for ProSe 583

7.6A Void 584

7.6B Blocking characteristics for UL-MIMO 584

7.7 Spurious response 584

7.7.1 Minimum requirements 584

7.7.1A Minimum requirements for CA 585

7.7.1B Minimum requirements for UL-MIMO 586

7.7.1D Minimum requirements for ProSe 586

7.7.1F Minimum requirements for UE category NB1 and NB2 587

7.7.1G Minimum requirements for V2X 587

7.8 Intermodulation characteristics 588

7.8.1 Wide band intermodulation 588

7.8.1.1 Minimum requirements 588

7.8.1A Minimum requirements for CA 589

7.8.1B Minimum requirements for UL-MIMO 592

7.8.1D Minimum requirements for ProSe 592

7.8.1F Minimum requirements for category NB1 and NB2 593

7.8.1G Minimum requirements 593

7.8.2 Void 594

7.9 Spurious emissions 594

7.9.1 Minimum requirements 595

7.9.1A Minimum requirements 595

7.10 Receiver image 596

7.10.1 Void 596

7.10.1A Minimum requirements for CA 596

7.10.1G Minimum requirements for V2X Communication 596

8 Performance requirement 643

8.1 General 643

8.1.1 Receiver antenna capability 643

8.1.1.1 Simultaneous unicast and MBMS operations 644

8.1.1.2 Dual-antenna receiver capability in idle mode 644

8.1.2 Applicability of requirements 644

8.1.2.1 Applicability of requirements for different channel bandwidths 644

8.1.2.2 Definition of CA capability 644

8.1.2.2A Definition of dual connectivity capability 649

8.1.2.3 Applicability and test rules for different CA configurations and bandwidth combination sets 650

8.1.2.3A Applicability and test rules for different dual connectivity configuration and bandwidth combination set 653

8.1.2.3B Applicability and test rules for different TDD-FDD CA configurations and bandwidth combination sets 654

8.1.2.3C Applicability and test rules for SDR tests for 4Rx capable UEs 656

8.1.2.3D Applicability and test rules for different CA with LAA SCell(s) configurations and bandwidth combination sets 656

8.1.2.3E Applicability and test rules for SDR tests for 8Rx capable UEs 657

8.1.2.4 Test coverage for different number of component carriers 658

8.1.2.5 Applicability of performance requirements for Type B receiver 659

8.1.2.6 Applicability of performance requirements for 4Rx capable UEs 659

8.1.2.6.1 Applicability rule and antenna connection for single carrier tests with 2Rx 659

8.1.2.6.2 Applicability rule and antenna connection for CA and DC tests with 2Rx 661

8.1.2.6.3 Applicability rule and antenna connection for single carrier tests with 4Rx 661

8.1.2.6.4 Applicability rule for 256QAM tests 662

8.1.2.6.5 Applicability rule and antenna connection for CA and DC tests with 4Rx 662

8.1.2.6.6 Applicability rule for Type C with 4Rx 666

8.1.2.6.7 Applicability rule for 1024QAM tests 666

8.1.2.7 Applicability of Enhanced Downlink Control Channel Performance Requirements 666

8.1.2.8 Applicability of performance requirements for CDM-multiplexed DM RS with interfering simultaneous transmission (FRC) with multiple CSI-RS configurations 668

8.1.2.8A Applicability of performance requirements for UE supporting coverage enhancement 668

8.1.2.9 Applicability of SDR requirements for CA and LAA 669

8.1.2.10 Applicability of performance requirements for Multi-user Superposed Transmission 670

8.1.2.11 Applicability CRS interference mitigation receivers performance requirements 670

8.1.2.12 Applicability of performance requirements for 8Rx capable UEs 671

8.1.2.12.1 Applicability rule and antenna connection for single carrier PDSCH tests 671

8.1.2.12.2 Applicability rule and antenna connection for control channel tests 677

8.1.2.12.3 Applicability rule and antenna connection for CA and DC tests 677

8.1.3 UE category and UE DL category 678

8.2 Demodulation of PDSCH (Cell-Specific Reference Symbols) 678

8.2.1 FDD (Fixed Reference Channel) 678

8.2.1.1 Single-antenna port performance 679

8.2.1.1.1 Minimum Requirement 679

8.2.1.1.2 Void 685

8.2.1.1.3 Void 685

8.2.1.1.4 Minimum Requirement 1 PRB allocation in presence of MBSFN 685

8.2.1.1.4A Minimum Requirement 1 PRB allocation in presence of FeMBMS Unicast-mixed Cell under CA 685

8.2.1.2 Transmit diversity performance 686

8.2.1.2.1 Minimum Requirement 2 Tx Antenna Port 686

8.2.1.2.2 Minimum Requirement 4 Tx Antenna Port 687

8.2.1.2.3 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS) 687

8.2.1.2.3A Minimum Requirement 2 Tx Antenna Ports (demodulation subframe overlaps with aggressor cell ABS and CRS assistance information are configured) 689

8.2.1.2.4 Enhanced Performance Requirement Type A - 2 Tx Antenna Ports with TM3 interference model 691

8.2.1.2.5 Enhanced Performance Requirement Type B - 2 Tx Antenna Ports with TM2 interference model 693

8.2.1.2.6 Enhanced Performance Requirement Type B - 2 Tx Antenna Ports with TM9 interference model 694

8.2.1.2.7 Minimum Requirement 2 Tx Antenna Port (Superposed transmission) 695

8.2.1.3 Open-loop spatial multiplexing performance 695

8.2.1.3.1 Minimum Requirement 2 Tx Antenna Port 695

8.2.1.3.1A Soft buffer management test 699

8.2.1.3.1B Enhanced Performance Requirement Type C –2Tx Antenna Ports 700

8.2.1.3.1C Enhanced Performance Requirement Type C - 2 Tx Antenna Ports with TM1 interference 701

8.2.1.3.2 Minimum Requirement 4 Tx Antenna Port 702

8.2.1.3.3 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS) 702

8.2.1.3.4 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS and CRS assistance information are configured) 706

8.2.1.3.5 Minimum Requirement 2 Tx Antenna Port (Superposed transmission) 708

8.2.1.3.6 Minimum Requirement 2 Tx Antenna Port (network-based CRS interference mitigation) 709

8.2.1.4 Closed-loop spatial multiplexing performance 710

8.2.1.4.1 Minimum Requirement Single-Layer Spatial Multiplexing 2 Tx Antenna Port 710

8.2.1.4.1A Minimum Requirement Single-Layer Spatial Multiplexing 4 Tx Antenna Port 711

8.2.1.4.1B Enhanced Performance Requirement Type A - Single-Layer Spatial Multiplexing 2 Tx Antenna Port with TM4 interference model 711

8.2.1.4.1C Minimum Requirement Single-Layer Spatial Multiplexing 2 Tx Antenna Ports (demodulation subframe overlaps with aggressor cell ABS and CRS assistance information are configured) 713

8.2.1.4.1D Enhanced Performance Requirement Type B - Single-layer Spatial Multiplexing 2 Tx Antenna Port with TM4 interference model 716

8.2.1.4.1E Minimum Requirement Single-Layer Spatial Multiplexing 2 Tx Antenna Ports with CRS assistance information 718

8.2.1.4.1F Minimum Requirement Single-Layer Spatial Multiplexing 4 Tx Antenna Ports with CRS assistance information 719

8.2.1.4.2 Minimum Requirement Multi-Layer Spatial Multiplexing 2 Tx Antenna Port 720

8.2.1.4.2A Enhanced Performance Requirement Type C – Multi-layer Spatial Multiplexing 2Tx Antenna Ports 721

8.2.1.4.3 Minimum Requirement Multi-Layer Spatial Multiplexing 4 Tx Antenna Port 721

8.2.1.4.3A Minimum Requirement Multi-Layer Spatial Multiplexing 4 Tx Antenna Port for dual connectivity 725

8.2.1.4.4 Minimum Requirement Multi-Layer Spatial Multiplexing 2 Tx Antenna Port (Superposed transmission) 727

8.2.1.5 MU-MIMO 728

8.2.1.6 [Control channel performance: D-BCH and PCH] 728

8.2.1.7 Carrier aggregation with power imbalance 728

8.2.1.7.1 Minimum Requirement 728

8.2.1.8 Intra-band non-contiguous carrier aggregation with timing offset 729

8.2.1.8.1 Minimum Requirement 729

8.2.1.9 HST-SFN performance 730

8.2.1.9.1 Minimum Requirement 730

8.2.1.9.2 Minimum Requirement for Rel-16 further enhanced HST 733

8.2.1.10 Intra-band contiguous carrier aggregation with minimum channel spacing 733

8.2.1.10.1 Minimum Requirement 734

8.2.2 TDD (Fixed Reference Channel) 734

8.2.2.1 Single-antenna port performance 735

8.2.2.1.1 Minimum Requirement 735

8.2.2.1.2 Void 740

8.2.2.1.3 Void 740

8.2.2.1.4 Minimum Requirement 1 PRB allocation in presence of MBSFN 740

8.2.2.2 Transmit diversity performance 740

8.2.2.2.1 Minimum Requirement 2 Tx Antenna Port 740

8.2.2.2.2 Minimum Requirement 4 Tx Antenna Port 741

8.2.2.2.3 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS) 742

8.2.2.2.3A Minimum Requirement 2 Tx Antenna Ports (demodulation subframe overlaps with aggressor cell ABS and CRS assistance information are configured) 743

8.2.2.2.4 Enhanced Performance Requirement Type A – 2 Tx Antenna Ports with TM3 interference model 745

8.2.2.2.5 Minimum Requirement 2 Tx Antenna Port (when *EIMTA-MainConfigServCell-r12* is configured) 747

8.2.2.2.6 Enhanced Performance Requirement Type B - 2 Tx Antenna Ports with TM2 interference model 747

8.2.2.2.7 Enhanced Performance Requirement Type B - 2 Tx Antenna Ports with TM9 interference model 749

8.2.2.2.8 Minimum Requirement 2 Tx Antenna Port (Superposed transmission) 750

8.2.2.3 Open-loop spatial multiplexing performance 751

8.2.2.3.1 Minimum Requirement 2 Tx Antenna Port 751

8.2.2.3.1A Soft buffer management test 754

8.2.2.3.1B Enhanced Performance Requirement Type C - 2Tx Antenna Ports 754

8.2.2.3.1C Enhanced Performance Requirement Type C - 2 Tx Antenna Ports with TM1 interference 755

8.2.2.3.2 Minimum Requirement 4 Tx Antenna Port 756

8.2.2.3.3 Minimum Requirement 2Tx antenna port (demodulation subframe overlaps with aggressor cell ABS) 757

8.2.2.3.4 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS and CRS assistance information are configured) 761

8.2.2.3.5 Minimum Requirement 2 Tx Antenna Port (Superposed transmission) 763

8.2.2.3.6 Minimum Requirement 2 Tx Antenna Port (network-based CRS interference mitigation) 764

8.2.2.4 Closed-loop spatial multiplexing performance 765

8.2.2.4.1 Minimum Requirement Single-Layer Spatial Multiplexing 2 Tx Antenna Port 765

8.2.2.4.1A Minimum Requirement Single-Layer Spatial Multiplexing 4 Tx Antenna Port 766

8.2.2.4.1B Enhanced Performance Requirement Type A – Single-Layer Spatial Multiplexing 2 Tx Antenna Port with TM4 interference model 766

8.2.2.4.1C Minimum Requirement Single-Layer Spatial Multiplexing 2 Tx Antenna Ports (demodulation subframe overlaps with aggressor cell ABS and CRS assistance information are configured) 768

8.2.2.4.1D Enhanced Performance Requirement Type B - Single-layer Spatial Multiplexing 2 Tx Antenna Port with TM4 interference model 770

8.2.2.4.1E Minimum Requirement Single-Layer Spatial Multiplexing 2 Tx Antenna Ports with CRS assistance information 772

8.2.2.4.1F Minimum Requirement Single-Layer Spatial Multiplexing 4 Tx Antenna Ports with CRS assistance information 773

8.2.2.4.2 Minimum Requirement Multi-Layer Spatial Multiplexing 2 Tx Antenna Port 775

8.2.2.4.2A Enhanced Performance Requirement Type C Multi-Layer Spatial Multiplexing 2 Tx Antenna Port 775

8.2.2.4.3 Minimum Requirement Multi-Layer Spatial Multiplexing 4 Tx Antenna Port 776

8.2.2.4.3A Minimum Requirement Multi-Layer Spatial Multiplexing 4 Tx Antenna Port for dual connectivity 780

8.2.2.4.4 Void 781

8.2.2.4.5 Minimum Requirement Multi-Layer Spatial Multiplexing 2 Tx Antenna Port (Superposed transmission) 781

8.2.2.5 MU-MIMO 782

8.2.2.6 [Control channel performance: D-BCH and PCH] 782

8.2.2.7 Carrier aggregation with power imbalance 782

8.2.2.7.1 Minimum Requirement 782

8.2.2.8 Intra-band contiguous carrier aggregation with minimum channel spacing 783

8.2.2.8.1 Minimum Requirement 783

8.2.2.9 HST-SFN performance 784

8.2.2.9.1 Minimum Requirement 784

8.2.2.9.2 Minimum Requirement for Rel-16 further enhanced HST 786

8.2.3 TDD FDD CA (Fixed Reference Channel) 787

8.2.3.1 Single-antenna port performance 788

8.2.3.1.1 Minimum Requirement for FDD PCell 788

8.2.3.1.2 Minimum Requirement for TDD PCell 792

8.2.3.2 Open-loop spatial multiplexing performance 2Tx Antenna port 796

8.2.3.2.1 Minimum Requirement for FDD PCell 796

8.2.3.2.1A Soft buffer management test for FDD PCell 800

8.2.3.2.2 Minimum Requirement for TDD PCell 801

8.2.3.2.2A Soft buffer management test for TDD PCell 805

8.2.3.3 Closed-loop spatial multiplexing performance 4Tx Antenna Port 806

8.2.3.3.1 Minimum Requirement for FDD PCell 806

8.2.3.3.2 Minimum Requirement for TDD PCell 810

8.2.3.4 Minimum Requirement for Closed-loop spatial multiplexing performance 4Tx Antenna Port for dual connectivity 814

8.2.3.5 HST-SFN performance 816

8.2.3.5.0 General 816

8.2.3.5.1 Minimum Requirement for FDD PCell 816

8.2.3.5.2 Minimum Requirement for TDD PCell 819

8.2.4 LAA 822

8.2.4.1 Closed-loop spatial multiplexing performance 4Tx Antenna Port 822

8.2.4.1.1 FDD PCell (FDD single carrier) 822

8.2.4.1.2 TDD PCell (TDD single carrier) 826

8.3 Demodulation of PDSCH (User-Specific Reference Symbols) 829

8.3.1 FDD 829

8.3.1.1 Single-layer Spatial Multiplexing 830

8.3.1.1A Enhanced Performance Requirement Type A – Single-layer Spatial Multiplexing with TM9 interference model 832

8.3.1.1B Single-layer Spatial Multiplexing (demodulation subframe overlaps with aggressor cell ABS and CRS assistance information are configured) 835

8.3.1.1C Enhanced Performance Requirement Type B – Single-layer Spatial Multiplexing with TM9 interference model 838

8.3.1.1D Enhanced Performance Requirement Type B – Single-layer Spatial Multiplexing with CRS interference model 840

8.3.1.1E Enhanced Performance Requirement Type B – Single-layer Spatial Multiplexing with TM3 interference model 841

8.3.1.1F Enhanced Performance Requirement Type B – Single-layer Spatial Multiplexing with TM10 serving cell configuration and TM9 interference model 842

8.3.1.1G Single-layer Spatial Multiplexing (CRS assistance information is configured) 844

8.3.1.1H Single-layer Spatial Multiplexing (With Enhanced DMRS table configured) 846

8.3.1.1I Single-layer Spatial Multiplexing (with assistance information for simultaneous transmition interfering PDSCH) 847

8.3.1.2 Dual-Layer Spatial Multiplexing 849

8.3.1.2A Enhanced Performance Requirement Type C - Dual-Layer Spatial Multiplexing 850

8.3.1.3 Performance requirements for DCI format 2D and non Quasi Co-located Antenna Ports 851

8.3.1.3.1 Minimum requirement with Same Cell ID (with single NZP CSI-RS resource) 851

8.3.1.3.2 Minimum requirements with Same Cell ID (with multiple NZP CSI-RS resources) 853

8.3.1.3.3 Minimum requirement with Different Cell ID and Colliding CRS (with single NZP CSI-RS resource) 855

8.3.1.3.4 Minimum requirement with Different Cell ID and non-colliding CRS (with single NZP CSI-RS resource and CRS assistance information is configured) 857

8.3.1.3.5 Minimum requirements with different Cell ID and non-colliding CRS (with multiple NZP CSI-RS resources and CRS assistance information is configured) 859

8.3.1.3.6 Minimum requirements for QCL Type C and 2 Layers Spatial Multiplexing 862

8.3.1.4 Performance Requirements for semiOpenLoop transmission 864

8.3.2 TDD 866

8.3.2.1 Single-layer Spatial Multiplexing 866

8.3.2.1A Single-layer Spatial Multiplexing (with multiple CSI-RS configurations) 868

8.3.2.1B Enhanced Performance Requirement Type A – Single-layer Spatial Multiplexing with TM9 interference model 870

8.3.2.1C Single-layer Spatial Multiplexing (demodulation subframe overlaps with aggressor cell ABS and CRS assistance information are configured) 873

8.3.2.1D Enhanced Performance Requirement Type B – Single-layer Spatial Multiplexing with TM9 interference 876

8.3.2.1E Enhanced Performance Requirement Type B – Single-layer Spatial Multiplexing with CRS interference model 878

8.3.2.1F Enhanced Performance Requirement Type B – Single-layer Spatial Multiplexing with TM3 interference 880

8.3.2.1G Enhanced Performance Requirement Type B – Single-layer Spatial Multiplexing with TM10 serving cell configuration and TM9 interference model 881

8.3.2.1H Single-layer Spatial Multiplexing (CRS assistance information is configured) 883

8.3.2.1I Single-layer Spatial Multiplexing (With Enhanced DMRS table configured) 885

8.3.2.1J Single-layer Spatial Multiplexing (with assistance information for simultaneous transmition interfering PDSCH) 886

8.3.2.2 Dual-Layer Spatial Multiplexing 888

8.3.2.2A Enhanced Performance Requirement Type C - Dual-Layer Spatial Multiplexing 888

8.3.2.3 Dual-Layer Spatial Multiplexing (with multiple CSI-RS configurations) 889

8.3.2.4 Performance requirements for DCI format 2D and non Quasi Co-located Antenna Ports 890

8.3.2.4.1 Minimum requirement with Same Cell ID (with single NZP CSI-RS resource) 890

8.3.2.4.2 Minimum requirements with Same Cell ID (with multiple NZP CSI-RS resources) 892

8.3.2.4.3 Minimum requirement with Different Cell ID and Colliding CRS (with single NZP CSI-RS resource) 894

8.3.2.4.4 Minimum requirement with Different Cell ID and non-Colliding CRS (with single NZP CSI-RS resource and CRS assistance information is configured) 896

8.3.2.4.5 Minimum requirements with different Cell ID and non-colliding CRS (with multiple NZP CSI-RS resources and CRS assistance information is configured) 898

8.3.2.4.6 Minimum requirements for QCL Type C and 2 Layers Spatial Multiplexing 901

8.3.2.5 Performance Requirements for semiOpenLoop transmission 903

8.3.3 LAA 905

8.3.3.1 Dual-Layer Spatial Multiplexing with DM-RS 905

8.3.3.1.1 FDD PCell (FDD single carrier) 905

8.3.3.1.2 TDD Pcell (TDD single carrier) 910

8.4 Demodulation of PDCCH/PCFICH 914

8.4.1 FDD 914

8.4.1.1 Single-antenna port performance 915

8.4.1.2 Transmit diversity performance 915

8.4.1.2.1 Minimum Requirement 2 Tx Antenna Port 915

8.4.1.2.2 Minimum Requirement 4 Tx Antenna Port 915

8.4.1.2.3 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS) 916

8.4.1.2.4 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS and CRS assistance information are configured) 921

8.4.1.2.5 Enhanced Downlink Control Channel Performance Requirement Type A - 2 Tx Antenna Port under Asynchronous Network 927

8.4.1.2.6 Enhanced Downlink Control Channel Performance Requirement Type A - 2 Tx Antenna Port with Non-Colliding CRS Dominant Interferer 928

8.4.1.2.7 Enhanced Downlink Control Channel Performance Requirement Type B - 2 Tx Antenna Port with Colliding CRS Dominant Interferer 929

8.4.1.2.8 Enhanced Downlink Control Channel Performance Requirement Type B - 2 Tx Antenna Port with Non-Colliding CRS Dominant Interferer 930

8.4.1.2.9 Enhanced Downlink Control Channel Performance Requirement Type A - 4 Tx Antenna Port with Non-Colliding CRS Dominant Interferer 931

8.4.2 TDD 932

8.4.2.1 Single-antenna port performance 933

8.4.2.2 Transmit diversity performance 933

8.4.2.2.1 Minimum Requirement 2 Tx Antenna Port 933

8.4.2.2.2 Minimum Requirement 4 Tx Antenna Port 934

8.4.2.2.3 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS) 934

8.4.2.2.4 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS and CRS assistance information are configured) 938

8.4.2.2.5 Enhanced Downlink Control Channel Performance Requirement Type A - 2 Tx Antenna Port with Colliding CRS Dominant Interferer 942

8.4.2.2.6 Enhanced Downlink Control Channel Performance Requirement Type A - 2 Tx Antenna Port with Non-Colliding CRS Dominant Interferer 943

8.4.2.2.7 Enhanced Downlink Control Channel Performance Requirement Type B - 2 Tx Antenna Port with Colliding CRS Dominant Interferer 944

8.4.2.2.8 Enhanced Downlink Control Channel Performance Requirement Type B - 2 Tx Antenna Port with Non-Colliding CRS Dominant Interferer 945

8.4.2.2.9 Enhanced Downlink Control Channel Performance Requirement Type A - 4 Tx Antenna Port with Non-Colliding CRS Dominant Interferer 946

8.4.3 LAA 947

8.4.3.1 Transmit diversity performance 947

8.4.3.1.1 FDD Pcell (FDD single carrier) 947

8.4.3.1.2 TDD Pcell (TDD single carrier) 948

8.5 Demodulation of PHICH 949

8.5.1 FDD 950

8.5.1.1 Single-antenna port performance 950

8.5.1.2 Transmit diversity performance 950

8.5.1.2.1 Minimum Requirement 2 Tx Antenna Port 950

8.5.1.2.2 Minimum Requirement 4 Tx Antenna Port 951

8.5.1.2.3 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS) 951

8.5.1.2.4 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS and CRS assistance information are configured) 953

8.5.1.2.5 Enhanced Downlink Control Channel Performance Requirement Type A - 2 Tx Antenna Ports under Asynchronous Network 956

8.5.1.2.6 Enhanced Downlink Control Channel Performance Requirement Type A - 2 Tx Antenna Ports with Non-Colliding CRS Dominant Interferer 957

8.5.1.2.7 Enhanced Downlink Control Channel Performance Requirement Type B - 2 Tx Antenna Ports with Colliding CRS Dominant Interferer 958

8.5.1.2.8 Enhanced Downlink Control Channel Performance Requirement Type B - 2 Tx Antenna Ports with Non-Colliding CRS Dominant Interferer 959

8.5.2 TDD 960

8.5.2.1 Single-antenna port performance 961

8.5.2.2 Transmit diversity performance 961

8.5.2.2.1 Minimum Requirement 2 Tx Antenna Port 961

8.5.2.2.2 Minimum Requirement 4 Tx Antenna Port 962

8.5.2.2.3 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS) 962

8.5.2.2.4 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS and CRS assistance information are configured) 964

8.5.2.2.5 Enhanced Downlink Control Channel Performance Requirement Type A - 2 Tx Antenna Ports with Colliding CRS Dominant Interferer 966

8.5.2.2.6 Enhanced Downlink Control Channel Performance Requirement Type A - 2 Tx Antenna Ports with Non-Colliding CRS Dominant Interferer 967

8.5.2.2.7 Enhanced Downlink Control Channel Performance Requirement Type B - 2 Tx Antenna Ports with Colliding CRS Dominant Interferer 968

8.5.2.2.8 Enhanced Downlink Control Channel Performance Requirement Type B - 2 Tx Antenna Ports with Non-Colliding CRS Dominant Interferer 969

8.6 Demodulation of PBCH 970

8.6.1 FDD 970

8.6.1.1 Single-antenna port performance 970

8.6.1.2 Transmit diversity performance 971

8.6.1.2.1 Minimum Requirement 2 Tx Antenna Port 971

8.6.1.2.2 Minimum Requirement 4 Tx Antenna Port 971

8.6.1.2.3 Minimum Requirement 2 Tx Antenna Port under Time Domain Measurement Resource Restriction with CRS Assistance Information 971

8.6.2 TDD 973

8.6.2.1 Single-antenna port performance 973

8.6.2.2 Transmit diversity performance 973

8.6.2.2.1 Minimum Requirement 2 Tx Antenna Port 973

8.6.2.2.2 Minimum Requirement 4 Tx Antenna Port 973

8.6.2.2.3 Minimum Requirement 2 Tx Antenna Port under Time Domain Measurement Resource Restriction with CRS Assistance Information 974

8.7 Sustained downlink data rate provided by lower layers 975

8.7.1 FDD (single carrier and CA) 975

8.7.2 TDD (single carrier and CA) 992

8.7.3 FDD (EPDCCH scheduling) 996

8.7.4 TDD (EPDCCH scheduling) 998

8.7.5 TDD FDD CA 1000

8.7.5.1 Minimum Requirement FDD PCell 1001

8.7.5.2 Minimum Requirement TDD PCell 1009

8.7.6 FDD (DC) 1018

8.7.7 TDD (DC) 1025

8.7.8 TDD FDD (DC) 1028

8.7.9 FDD (4 Rx) 1031

8.7.10 TDD (4 Rx) 1033

8.7.11 TDD FDD CA (4 Rx) 1035

8.7.11.1 Void 1037

8.7.12 LAA 1037

8.7.12.1 FDD CA in licensed bands 1037

8.7.12.2 TDD CA in licensed bands 1039

8.7.12.3 TDD-FDD CA in licensed bands 1041

8.7.13 FDD DC (4 Rx) 1044

8.7.14 TDD DC (4 Rx) 1045

8.7.15 TDD FDD DC (4 Rx) 1047

8.7.16 FDD (1024QAM and up to 4Rx supported) 1049

8.7.17 TDD (1024QAM and up to 4 Rx supported) 1052

8.7.18 TDD FDD CA (1024QAM and up to 4 Rx supported) 1054

8.7.19 TDD (8 Rx) 1056

8.8 Demodulation of EPDCCH 1058

8.8.1 Distributed Transmission 1058

8.8.1.1 FDD 1058

8.8.1.1.1 Void 1059

8.8.1.2 TDD 1059

8.8.1.2.1 Void 1060

8.8.2 Localized Transmission with TM9 1060

8.8.2.1 FDD 1060

8.8.2.1.1 Void 1061

8.8.2.1.2 Void 1062

8.8.2.2 TDD 1062

8.8.2.2.1 Void 1063

8.8.2.2.2 Void 1063

8.8.3 Localized transmission with TM10 Type B quasi co-location type 1063

8.8.3.1 FDD 1063

8.8.3.2 TDD 1066

8.8.4 Enhanced Downlink Control Channel Performance Requirements Type A - Localized Transmission with CRS Interference Model 1069

8.8.4.1 FDD 1069

8.8.4.2 TDD 1070

8.8.5 Enhanced Downlink Control Channel Performance Requirements Type A - Distributed Transmission with TM9 Interference Model 1072

8.8.5.1 TDD 1072

8.8.6 Enhanced Downlink Control Channel Performance Requirements Type A - Distributed Transmission with TM3 Interference Model 1073

8.8.6.1 FDD 1073

8.9 Demodulation (single receiver antenna) 1074

8.9.1 PDSCH 1074

8.9.1.1 FDD and half-duplex FDD (Fixed Reference Channel) 1074

8.9.1.1.1 Transmit diversity performance (Cell-Specific Reference Symbols) 1074

8.9.1.1.2 Closed-loop spatial multiplexing performance (Cell-Specific Reference Symbols) 1075

8.9.1.1.3 Closed-loop spatial multiplexing performance (User-Specific Reference Symbols) 1077

8.9.1.2 TDD (Fixed Reference Channel) 1080

8.9.1.2.1 Transmit diversity performance (Cell-Specific Reference Symbols) 1080

8.9.1.2.2 Closed-loop spatial multiplexing performance (Cell-Specific Reference Symbols) 1081

8.9.1.2.3 Closed-loop spatial multiplexing performance (User-Specific Reference Symbols) 1084

8.9.2 PHICH 1086

8.9.2.1 FDD and half-duplex FDD 1086

8.9.2.1.1 Transmit diversity performance 1086

8.9.2.2 TDD 1086

8.9.2.2.1 Transmit diversity performance 1086

8.9.3 PBCH 1087

8.9.3.1 FDD and half-duplex FDD 1087

8.9.3.1.1 Transmit diversity performance 1087

8.9.3.2 TDD 1087

8.9.3.2.1 Transmit diversity performance 1087

8.9.4 PDCCH/PCFICH 1087

8.9.4.1 FDD and half-duplex FDD 1087

8.9.4.1.1 Enhanced Downlink Control Channel Performance Requirement Type A - 2 Tx Antenna Port with Non-Colliding CRS Dominant Interferer 1087

8.9.4.1.2 Enhanced Downlink Control Channel Performance Requirement Type A - 4 Tx Antenna Port with Non-Colliding CRS Dominant Interferer 1088

8.9.4.2 TDD 1089

8.9.4.2.1 Enhanced Downlink Control Channel Performance Requirement Type A - 2 Tx Antenna Port with Non-Colliding CRS Dominant Interferer 1089

8.9.4.2.2 Enhanced Downlink Control Channel Performance Requirement Type A - 4 Tx Antenna Port with Non-Colliding CRS Dominant Interferer 1090

8.10 Demodulation (4 receiver antenna ports) 1091

8.10.1 PDSCH 1091

8.10.1.1 FDD (Fixed Reference Channel) 1091

8.10.1.1.1 Transmit diversity performance with 2Tx Antenna Ports (Cell-Specific Reference Symbols) 1092

8.10.1.1.1A Transmit diversity performance wit Enhanced Performance Requirement Type A - 2 Tx Antenna Ports with TM3 interference model 1093

8.10.1.1.2 Open-loop spatial multiplexing performance with 2Tx Antenna Ports (Cell-Specific Reference Symbols) 1094

8.10.1.1.3 Closed-loop spatial multiplexing Enhanced Performance Requirements Type A - Single-Layer Spatial Multiplexing 2 Tx Antenna Port with TM4 interference model (Cell-Specific Reference Symbols) 1094

8.10.1.1.4 Closed-loop spatial multiplexing performance, Dual-Layer Spatial Multiplexing 4 Tx Antenna Port (Cell-Specific Reference Symbols) 1095

8.10.1.1.4A Enhanced Performance Requirement Type C - Dual-Layer Spatial Multiplexing with 2Tx Antenna Ports 1096

8.10.1.1.5 Enhanced Performance Requirement Type A – Single-layer Spatial Multiplexing with TM9 interference model (User-Specific Reference Symbols) 1097

8.10.1.1.5A Single-layer Spatial Multiplexing (User-Specific Reference Symbols) 1100

8.10.1.1.5B Single-layer Spatial Multiplexing (With Enhanced DMRS table configured) 1101

8.10.1.1.6 Dual-Layer Spatial Multiplexing (User-Specific Reference Symbols) 1102

8.10.1.1.6A Enhanced Performance Requirement Type C - Dual-Layer Spatial Multiplexing 1104

8.10.1.1.6B Dual-Layer Spatial Multiplexing with altCQI-Table-1024QAM configured (User-Specific Reference Symbols) 1105

8.10.1.1.7 Open-loop spatial multiplexing, 3 Layer Multiplexing with 4 Tx Antenna Ports (Cell-Specific Reference Symbols) 1106

8.10.1.1.7A Enhanced Performance Requirement Type C - Open-loop spatial multiplexing, 3 Layer Multiplexing with 4 Tx Antenna Ports (Cell-Specific Reference Symbols) 1106

8.10.1.1.8 Closed-loop spatial multiplexing performance, 4 Layers spatial multiplexing 4 Tx antennas (Cell-Specific Reference Symbols) 1107

8.10.1.1.9 4 Layer Spatial Multiplexing (User-Specific Reference Symbols) 1107

8.10.1.1.9A Enhanced Performance Requirement Type C - 4 Layer Spatial Multiplexing (User-Specific Reference Symbols) 1109

8.10.1.1.10 Closed loop spatial multiplexing performance - Single-Layer Spatial Multiplexing 2 Tx Antenna Port with CRS assistance information (Cell-Specific Reference Symbols) 1110

8.10.1.1.11 Closed loop spatial multiplexing performance - Single-Layer Spatial Multiplexing 4 Tx Antenna Port with CRS assistance information (Cell-Specific Reference Symbols) 1111

8.10.1.1.12 Closed loop spatial multiplexing performance - Single-Layer Spatial Multiplexing with CRS assistance information (User-Specific Reference Symbols) 1112

8.10.1.1.13 Performance requirements for DCI format 2D and non Quasi Co-located Antenna Ports 1113

8.10.1.1.14 HST-SFN performance 1117

8.10.1.2 TDD (Fixed Reference Channel) 1117

8.10.1.2.1 Transmit diversity performance with 2Tx Antenna Ports (Cell-Specific Reference Symbols) 1118

8.10.1.2.1A Transmit diversity performance with Enhanced Performance Requirement Type A – 2 Tx Antenna Ports with TM3 interference model 1119

8.10.1.2.2 Open-loop spatial multiplexing performance with 2Tx Antenna Ports (Cell-Specific Reference Symbols) 1120

8.10.1.2.3 Closed-loop spatial multiplexing Enhanced Performance Requirements Type A - Single-Layer Spatial Multiplexing 2 Tx Antenna Port with TM4 interference model (Cell-Specific Reference Symbols) 1120

8.10.1.2.4 Closed-loop spatial multiplexing performance, Dual-Layer Spatial Multiplexing 4 Tx Antenna Ports (Cell-Specific Reference Symbols) 1121

8.10.1.2.4A Enhanced Performance Requirement Type C - Dual-Layer Spatial Multiplexing with 2Tx Antenna Ports 1122

8.10.1.2.5 Enhanced Performance Requirement Type A – Single-layer Spatial Multiplexing with TM9 interference model (User-Specific Reference Symbols) 1123

8.10.1.2.5A Single-layer Spatial Multiplexing (with multiple CSI-RS configurations) 1126

8.10.1.2.5B Single-layer Spatial Multiplexing (With Enhanced DMRS table configured) 1127

8.10.1.2.6 Dual-Layer Spatial Multiplexing (User-Specific Reference Symbols) 1128

8.10.1.2.6A Enhanced Performance Requirement Type C - Dual-Layer Spatial Multiplexing 1130

8.10.1.2.6B Dual-Layer Spatial Multiplexing with altCQI-Table-1024QAM configured (User-Specific Reference Symbols) 1131

8.10.1.2.7 Open-loop spatial multiplexing, 3 Layer Multiplexing with 4 Tx Antenna Ports (Cell-Specific Reference Symbols) 1132

8.10.1.2.7A Enhanced Performance Requirement Type C - Open-loop spatial multiplexing, 3 Layer Multiplexing with 4 Tx Antenna Ports (Cell-Specific Reference Symbols) 1132

8.10.1.2.8 Closed-loop spatial multiplexing performance, 4 Layers spatial multiplexing 4 Tx antennas 1133

8.10.1.2.9 4 Layer Spatial Multiplexing (User-Specific Reference Symbols) 1134

8.10.1.2.9A Enhanced Performance Requirement Type C - 4 Layer Spatial Multiplexing (User-Specific Reference Symbols) 1135

8.10.1.2.10 Closed loop spatial multiplexing performance - Single-Layer Spatial Multiplexing 2 Tx Antenna Port with CRS assistance information (Cell-Specific Reference Symbols) 1136

8.10.1.2.11 Closed loop spatial multiplexing performance - Single-Layer Spatial Multiplexing 4 Tx Antenna Port with CRS assistance information (Cell-Specific Reference Symbols) 1138

8.10.1.2.12 Closed loop spatial multiplexing performance - Single-Layer Spatial Multiplexing with CRS assistance information (User-Specific Reference Symbols) 1139

8.10.1.2.13 Performance requirements for DCI format 2D and non Quasi Co-located Antenna Ports 1141

8.10.1.2.14 HST-SFN performance 1145

8.10.2 PDCCH/PCFICH 1146

8.10.2.1 FDD 1146

8.10.2.1.1 Single-antenna port performance 1146

8.10.2.1.2 Transmit diversity performance with 2 Tx Antenna Ports 1146

8.10.2.1.3 Transmit diversity performance with 4 Tx Antenna Ports 1146

8.10.2.1.4 Enhanced Downlink Control Channel Performance Requirement Type A - 4 Tx Antenna Port with Non-Colliding CRS Dominant Interferer 1147

8.10.2.2 TDD 1148

8.10.2.2.1 Single-antenna port performance 1148

8.10.2.2.2 Transmit diversity performance with 2 Tx Antenna Ports 1149

8.10.2.2.3 Transmit diversity performance with 4 Tx Antenna Ports 1149

8.10.2.2.4 Enhanced Downlink Control Channel Performance Requirement Type A - 4 Tx Antenna Port with Non-Colliding CRS Dominant Interferer 1149

8.10.3 PHICH 1150

8.10.3.1 FDD 1150

8.10.3.1.1 Single Tx Antenna Port performance 1151

8.10.3.1.2 Transmit diversity performance with 2 Tx Antenna Ports 1151

8.10.3.1.3 Transmit diversity performance with 4 Tx Antenna Ports 1151

8.10.3.2 TDD 1152

8.10.3.2.1 Single Tx Antenna Port performance 1152

8.10.3.2.2 Transmit diversity performance with 2 Tx Antenna Ports 1153

8.10.3.2.3 Transmit diversity performance with 4 Tx Antenna Ports 1153

8.10.4 ePDCCH 1153

8.10.4.1 Distributed Transmission with 4Rx 1153

8.10.4.1.1 FDD 1153

8.10.4.1.2 TDD 1154

8.10.4.2 Localized Transmission with TM9 and 4Rx 1155

8.10.4.2.1 FDD 1155

8.10.4.2.2 TDD 1156

8.11 Demodulation (UE supporting coverage enhancement) 1157

8.11.1 PDSCH 1158

8.11.1.1 FDD and half-duplex FDD (Fixed Reference Channel) 1158

8.11.1.1.1 Closed-loop spatial multiplexing performance (Cell-Specific Reference Symbols) 1158

8.11.1.1.2 Closed-loop spatial multiplexing performance (User-Specific Reference Symbols) 1162

8.11.1.1.3 Transmit diversity performance (Cell-Specific Reference Symbols) 1164

8.11.1.2 TDD (Fixed Reference Channel) 1170

8.11.1.2.1 Closed-loop spatial multiplexing performance (Cell-Specific Reference Symbols) 1170

8.11.1.2.2 Closed-loop spatial multiplexing performance (User-Specific Reference Symbols) 1175

8.11.1.2.3 Transmit diversity performance (Cell-Specific Reference Symbols) 1177

8.11.2 MPDCCH 1181

8.11.2.1 FDD and half-duplex FDD 1182

8.11.2.1.1 CE Mode A 1183

8.11.2.1.2 CE Mode B 1184

8.11.2.1.3 CE Mode A with TM9 interference model 1184

8.11.2.1.4 CE Mode A with CRS interference model 1186

8.11.2.1.5 CE Mode A and CE Mode B when CRS-ChEstMPDCCH-Config is configured 1187

8.11.2.2.5 CE Mode A and CE Mode B when CRS-ChEstMPDCCH-Config is configured 1188

8.11.2.2 TDD 1190

8.11.2.2.1 CE Mode A 1191

8.11.2.2.2 CE Mode B 1192

8.11.2.2.3 CE Mode A with TM9 interference model 1192

8.11.2.2.4 CE Mode A with CRS interference model 1193

8.11.3 PBCH 1194

8.11.3.1 FDD and half-duplex FDD 1195

8.11.3.1.1 Transmit diversity performance 1195

8.11.3.2 TDD 1196

8.11.3.2.1 Transmit diversity performance 1196

8.12 Demodulation of Narrowband IoT 1196

8.12.1 NPDSCH 1196

8.12.1.1.1 Minimum Requirements for In-band 1197

8.12.1.1.2 Minimum Requirements for Standalone/Guard-band 1198

8.12.1.1.3 Minimum Requirements for Standalone for UE Category NB2 1199

8.12.1.1.4 Minimum Requirements for Standalone for UE with multiple TBs interleaved transmission 1200

8.12.1.1.5 Minimum Requirements for Standalone for UE with 16-QAM 1200

8.12.1.2 TDD 1202

8.12.1.2.1 Minimum Requirements for In-band 1202

8.12.1.2.2 Minimum Requirements for Standalone/Guard-band 1203

8.12.1.2.3 Minimum Requirements for Standalone for UE Category NB2 1204

8.12.1.2.4 Minimum Requirements for Standalone for UE with 16-QAM 1204

8.12.2 NPDCCH 1205

8.12.2.1 Half-duplex FDD 1205

8.12.2.1.1 Single-antenna performance 1206

8.12.2.1.2 Transmit diversity performance 1207

8.12.2.2 TDD 1207

8.12.2.2.1 Single-antenna performance 1209

8.12.2.2.2 Transmit diversity performance 1209

8.12.3 Demodulation of NPBCH 1209

8.12.3.1 HD-FDD 1210

8.12.3.1.1 Single-antenna port performance with single NPBCH TTI 1210

8.12.3.1.2 Transmit diversity performance 1210

8.12.3.2 TDD 1210

8.12.3.2.1 Single-antenna port performance with single NPBCH TTI 1211

8.12.3.2.2 Transmit diversity performance 1211

8.13 Demodulation of PDSCH CA and DC(4 receiver antenna ports) 1211

8.13.1 FDD (CA and DC) 1211

8.13.1.1 Closed-loop spatial multiplexing performance 1211

8.13.1.1.1 Minimum Requirement Multi-Layer Spatial Multiplexing 4 Tx Antenna Port 1211

8.13.1.1.2 Minimum Requirement Multi-Layer Spatial Multiplexing 4 Tx Antenna Port for dual connectivity 1215

8.13.1.1.3 Minimum Requirement Multi-Layer Spatial Multiplexing 4 Tx Antenna Port with 256QAM 1217

8.13.1.1.4 Minimum Requirement Four-Layer Spatial Multiplexing 4 Tx Antenna Port 1219

8.13.1.2 Dual-Layer Spatial Multiplexing (User-Specific Reference Symbols) 1220

8.13.1.2.1 Minimum Requirement Dual-Layer Spatial Multiplexing 2 Tx Antenna Port 1220

8.13.1.3 Enhanced Performance Requirements Type A Closed-loop spatial multiplexing 1223

8.13.1.3.1 Minimum Requirement Single-Layer Spatial Multiplexing 2 Tx Antenna Port with TM4 interference model (Cell-Specific Reference Symbols) 1223

8.13.1.4 Enhanced Performance Requirement Type A - Single-layer Spatial Multiplexing (User-Specific Reference Symbols) 1225

8.13.1.4.1 Minimum Requirement Enhanced Performance Requirement Type A – Single-layer Spatial Multiplexing with TM9 interference model (User-Specific Reference Symbols) 1225

8.13.2 TDD (CA and DC) 1228

8.13.2.1 Closed-loop spatial multiplexing performance 1229

8.13.2.1.1 Minimum Requirement Multi-Layer Spatial Multiplexing 4 Tx Antenna Port 1229

8.13.2.1.2 Minimum Requirement Multi-Layer Spatial Multiplexing 4 Tx Antenna Port for dual connectivity 1231

8.13.2.1.3 Minimum Requirement Multi-Layer Spatial Multiplexing 4 Tx Antenna Port with 256QAM 1232

8.13.2.1.4 Minimum Requirement Four-Layer Spatial Multiplexing 4 Tx Antenna Port 1233

8.13.2.2 Dual-Layer Spatial Multiplexing (User-Specific Reference Symbols) 1235

8.13.2.2.1 Minimum Requirement Dual-Layer Spatial Multiplexing 2 Tx Antenna Port 1235

8.13.2.4 Enhanced Performance Requirement Type A - Single-layer Spatial Multiplexing (User-Specific Reference Symbols) 1239

8.13.2.4.1 Minimum Requirement Enhanced Performance Requirement Type A – Single-layer Spatial Multiplexing with TM9 interference model (User-Specific Reference Symbols) 1239

8.13.3 TDD-FDD (CA and DC) 1241

8.13.3.1 Closed-loop spatial multiplexing performance 4Tx Antenna Port 1241

8.13.3.1.1 Minimum Requirement for FDD PCell 1241

8.13.3.1.2 Minimum Requirement for TDD PCell 1245

8.13.3.2 Dual-Layer Spatial Multiplexing (User-Specific Reference Symbols) 1249

8.13.3.2.1 Minimum Requirement Dual-Layer Spatial Multiplexing 2 Tx Antenna Port for FDD PCell 1249

8.13.3.2.2 Minimum Requirement Dual-Layer Spatial Multiplexing 2 Tx Antenna Port for TDD PCell 1252

8.13.3.3 Enhanced Performance Requirements Type A Closed-loop spatial multiplexing 1255

8.13.3.3.1 Minimum Requirement Single-Layer Spatial Multiplexing 2 Tx Antenna Port with TM4 interference model (Cell-Specific Reference Symbols) for FDD PCell 1255

8.13.3.3.2 Minimum Requirement Single-Layer Spatial Multiplexing 2 Tx Antenna Port with TM4 interference model (Cell-Specific Reference Symbols) for TDD PCell 1257

8.13.3.4 Enhanced Performance Requirement Type A - Single-layer Spatial Multiplexing (User-Specific Reference Symbols) 1259

8.13.3.4.1 Minimum Requirement Enhanced Performance Requirement Type A – Single-layer Spatial Multiplexing with TM9 interference model (User-Specific Reference Symbols) for FDD PCell 1259

8.13.3.4.2 Minimum Requirement Enhanced Performance Requirement Type A – Single-layer Spatial Multiplexing with TM9 interference model (User-Specific Reference Symbols) for TDD PCell 1262

8.13.3.5 Closed-loop spatial multiplexing performance 4Tx Antenna Port for DC 1265

8.13.3.5.1 Minimum Requirement for FDD PCell 1265

8.13.3.5.2 Minimum Requirement for TDD PCell 1267

8.13.3.6 Closed-loop spatial multiplexing performance 4Tx Antenna Port with 256QAM 1269

8.13.3.6.1 Minimum Requirement for FDD PCell 1269

8.13.3.6.2 Minimum Requirement for TDD PCell 1271

8.13.3.7 Closed-loop spatial multiplexing performance 4Tx Antenna Port with Four layers 1272

8.13.3.7.1 Minimum Requirement for FDD PCell 1272

8.13.3.7.2 Minimum Requirement for TDD PCell 1274

8.14 Demodulation (UE supporting Short TTI) 1276

8.14.1 Slot-PDSCH and Subslot-PDSCH 1276

8.14.1.1 FDD (Fixed Reference Channel) 1276

8.14.1.1.1 Open-loop spatial multiplexing performance 1276

8.14.1.1.2 Closed-loop spatial multiplexing performance (User-Specific Reference Signals) 1277

8.14.1.2 TDD (Fixed Reference Channel) 1279

8.14.1.2.1 Open-loop spatial multiplexing performance 1279

8.14.1.2.2 Closed-loop spatial multiplexing performance (User-Specific Reference Signals) 1280

8.14.2 SPDCCH 1281

8.14.2.1 FDD 1281

8.14.2.1.1 Mimimum requirement 1282

8.14.2.2 TDD 1282

8.14.2.2.1 Mimimum requirement 1283

8.15 Demodulation (8 receiver antenna ports) 1284

8.15.1 PDSCH 1284

8.15.1.1 Void 1284

8.15.1.2 TDD (Fixed Reference Channel) 1284

8.15.1.2.1 Transmit diversity performance with 2Tx Antenna Ports (Cell-Specific Reference Symbols) 1284

8.15.1.2.2 Open-loop spatial multiplexing performance with 2Tx Antenna Ports (Cell-Specific Reference Symbols) 1285

8.15.1.2.3 8 Layer Spatial Multiplexing (User-Specific Reference Symbols) 1285

8.15.2 CA 1287

8.15.2.1 Void 1287

8.15.2.2 TDD 1287

8.15.2.2.1 Eight Layer Spatial Multiplexing (User-Specific Reference Symbols) 1287

9 Reporting of Channel State Information 1289

9.1 General 1289

9.1.1 Applicability of requirements 1289

9.1.1.1 Applicability of requirements for different channel bandwidths 1289

9.1.1.2 Applicability and test rules for different CA configurations and bandwidth combination sets 1289

9.1.1.2A Applicability and test rules for different TDD-FDD CA configurations and bandwidth combination sets 1290

9.1.1.3 Test coverage for different number of componenet carriers 1291

9.1.1.4 Applicability of performance requirements for 4Rx capable UEs 1291

9.1.1.4.1 Applicability rule and antenna connection for single carrier tests with 2Rx 1291

9.1.1.4.2 Applicability rule and antenna connection for CA tests with 2Rx 1293

9.1.1.4.3 Applicability rule and antenna connection for single carrier tests with 4Rx 1294

9.1.1.5 Applicability of requirements for UEs supporting coverage enhancement 1294

9.2 CQI reporting definition under AWGN conditions 1294

9.2.1 Minimum requirement PUCCH 1-0 (Cell-Specific Reference Symbols) 1294

9.2.1.1 FDD 1294

9.2.1.2 TDD 1295

9.2.1.3 FDD (CSI measurements in case two CSI subframe sets are configured) 1296

9.2.1.4 TDD (CSI measurements in case two CSI subframe sets are configured) 1299

9.2.1.5 FDD (CSI measurements in case two CSI subframe sets are configured and with CRS assistance information) 1302

9.2.1.6 TDD (CSI measurements in case two CSI subframe sets are configured and with CRS assistance information) 1305

9.2.1.7 FDD (Modulation and TBS index Table 2 and 4-bit CQI Table 2 are used) 1308

9.2.1.8 TDD (Modulation and TBS index Table 2 and 4-bit CQI Table 2 are used) 1309

9.2.1.9 FDD (Modulation and TBS index Table 3 and 4-bit CQI Table 4 are used) 1309

9.2.1.10 TDD (Modulation and TBS index Table 3 and 4-bit CQI Table 4 are used) 1310

9.2.2 Minimum requirement PUCCH 1-1 (Cell-Specific Reference Symbols) 1311

9.2.2.1 FDD 1311

9.2.2.2 TDD 1312

9.2.3 Minimum requirement PUCCH 1-1 (CSI Reference Symbols) 1313

9.2.3.1 FDD 1313

9.2.3.1A FDD (With *channelMeasRestriction* configured) 1314

9.2.3.2 TDD 1315

9.2.3.2A TDD (With *channelMeasRestriction* configured) 1316

9.2.4 Minimum requirement PUCCH 1-1 (With Single CSI Process) 1317

9.2.4.1 FDD 1318

9.2.4.1A FDD (With *interferenceMeasRestriction* configured) 1320

9.2.4.2 TDD 1323

9.2.4.2A TDD (With *interferenceMeasRestriction* configured) 1326

9.2.5 Minimum requirement PUCCH 1-1 (when *csi-SubframeSet –r12* and *EIMTA-MainConfigServCell-r12* are configured) 1329

9.2.6 Minimum requirement PUSCH 3-0 (Cell-Specific Reference Symbols) 1332

9.2.6.1 Frame structure type 3 with FDD Pcell 1332

9.2.6.2 Frame structure type 3 with TDD Pcell 1334

9.2.7 Minimum requirement PUSCH 3-1 (CSI Reference Symbol) 1336

9.2.7.1 Frame structure type 3 wth FDD Pcell 1336

9.2.7.2 Frame structure type 3 wth TDD Pcell 1338

9.3 CQI reporting under fading conditions 1342

9.3.1 Frequency-selective scheduling mode 1342

9.3.1.1 Minimum requirement PUSCH 3-0 (Cell-Specific Reference Symbols) 1342

9.3.1.1.1 FDD 1342

9.3.1.1.2 TDD 1343

9.3.1.1.3 FDD (CSI measurements in case two CSI subframe sets are configured and with CRS assistance information) 1344

9.3.1.1.4 TDD (CSI measurements in case two CSI subframe sets are configured and with CRS assistance information) 1348

9.3.1.1.5 TDD (when *csi-SubframeSet –r12* is configured) 1351

9.3.1.2 Minimum requirement PUSCH 3-1 (CSI Reference Symbol) 1353

9.3.1.2.1 FDD 1353

9.3.1.2.2 TDD 1354

9.3.1.2.3 FDD (Modulation and TBS index Table 2 and 4-bit CQI Table 2 are used) 1356

9.3.1.2.4 TDD (Modulation and TBS index Table 2 and 4-bit CQI Table 2 are used) 1357

9.3.1.2.5 Void 1358

9.3.1.2.6 TDD (when *csi-SubframeSet –r12* is configured with one CSI process) 1358

9.3.2 Frequency non-selective scheduling mode 1362

9.3.2.1 Minimum requirement PUCCH 1-0 (Cell-Specific Reference Symbol) 1362

9.3.2.1.1 FDD 1362

9.3.2.1.2 TDD 1364

9.3.2.2 Minimum requirement PUCCH 1-1 (CSI Reference Symbol) 1366

9.3.2.2.1 FDD 1366

9.3.2.2.2 TDD 1367

9.3.3 Frequency-selective interference 1369

9.3.3.1 Minimum requirement PUSCH 3-0 (Cell-Specific Reference Symbol) 1369

9.3.3.1.1 FDD 1369

9.3.3.1.2 TDD 1370

9.3.3.2 Void 1371

9.3.3.2.1 Void 1371

9.3.3.2.2 Void 1371

9.3.4 UE-selected subband CQI 1371

9.3.4.1 Minimum requirement PUSCH 2-0 (Cell-Specific Reference Symbols) 1371

9.3.4.1.1 FDD 1371

9.3.4.1.2 TDD 1372

9.3.4.2 Minimum requirement PUCCH 2-0 (Cell-Specific Reference Symbols) 1373

9.3.4.2.1 FDD 1373

9.3.4.2.2 TDD 1375

9.3.5 Additional requirements for enhanced receiver Type A 1377

9.3.5.1 Minimum requirement PUCCH 1-0 (Cell-Specific Reference Symbol) 1377

9.3.5.1.1 FDD 1377

9.3.5.1.2 TDD 1378

9.3.5.2 Minimum requirement PUCCH 1-1 (CSI Reference Symbol) 1380

9.3.5.2.1 FDD 1380

9.3.5.2.2 TDD 1383

9.3.6 Minimum requirement (With multiple CSI processes) 1386

9.3.6.1 FDD 1387

9.3.6.2 TDD 1391

9.3.7 Minimum requirement PUSCH 3-2 1395

9.3.7.1 FDD 1395

9.3.7.2 TDD 1396

9.3.8 Additional requirements for enhanced receiver Type B 1398

9.3.8.1 Minimum requirement PUCCH 1-1 (Cell-Specific Reference Symbols) 1398

9.3.8.1.1 FDD 1398

9.3.8.1.2 TDD 1399

9.3.8.2 Minimum requirement PUCCH 1-1 (CSI Reference Symbols) 1401

9.3.8.2.1 FDD 1401

9.3.8.2.2 TDD 1403

9.3.8.3 Minimum requirement with CSI process 1406

9.3.8.3.1 FDD 1406

9.3.8.3.2 TDD 1409

9.4 Reporting of Precoding Matrix Indicator (PMI) 1412

9.4.1 Single PMI 1413

9.4.1.1 Minimum requirement PUSCH 3-1 (Cell-Specific Reference Symbols) 1413

9.4.1.1.1 FDD 1413

9.4.1.1.2 TDD 1414

9.4.1.2 Minimum requirement PUCCH 2-1 (Cell-Specific Reference Symbols) 1415

9.4.1.2.1 FDD 1415

9.4.1.2.2 TDD 1417

9.4.1.3 Minimum requirement PUSCH 3-1 (CSI Reference Symbol) 1418

9.4.1.3.1 FDD 1418

9.4.1.3.2 TDD 1421

9.4.1.3.3 FDD (with Class A 12Tx codebook) 1424

9.4.1.3.4 TDD (with Class A 12Tx codebook) 1426

9.4.1.3.5 FDD (with Class A 24Tx codebook) 1429

9.4.1.3.6 TDD (with Class A 24Tx codebook) 1431

9.4.1.4 Minimum requirement PUCCH 1-1 (CSI Reference Symbol) 1434

9.4.1.4.1 FDD (with 4Tx enhanced codebook) 1434

9.4.1.4.2 TDD (with 4Tx enhanced codebook) 1436

9.4.1.4.3 FDD (with Class B alternative codebook for one CSI-RS resource configured) 1439

9.4.1.4.4 TDD (with Class B alternative codebook for one CSI-RS resource configured) 1441

9.4.1a Void 1444

9.4.1a.1 Void 1444

9.4.1a.1.1 Void 1444

9.4.1a.1.2 Void 1444

9.4.2 Multiple PMI 1444

9.4.2.1 Minimum requirement PUSCH 1-2 (Cell-Specific Reference Symbols) 1444

9.4.2.1.1 FDD 1444

9.4.2.1.2 TDD 1445

9.4.2.2 Minimum requirement PUSCH 2-2 (Cell-Specific Reference Symbols) 1446

9.4.2.2.1 FDD 1446

9.4.2.2.2 TDD 1447

9.4.2.3 Minimum requirement PUSCH 1-2 (CSI Reference Symbol) 1448

9.4.2.3.1 FDD 1448

9.4.2.3.2 TDD 1450

9.4.2.3.3 FDD (with 4Tx enhanced codebook) 1453

9.4.2.3.4 TDD (with 4Tx enhanced codebook) 1455

9.4.2.3.5 FDD (with Class A 16Tx codebook) 1457

9.4.2.3.6 TDD (with Class A 16Tx codebook) 1460

9.4.2.3.7 FDD (with Class A 32Tx codebook) 1463

9.4.2.3.8 TDD (with Class A 32Tx codebook) 1466

9.4.2.3.9 FDD (with Class A 16Tx advanced codebook) 1469

9.4.2.3.10 TDD (with Class A 16Tx advanced codebook) 1472

9.4.3 Void 1475

9.5 Reporting of Rank Indicator (RI) 1475

9.5.1 Minimum requirement (Cell-Specific Reference Symbols) 1475

9.5.1.1 FDD 1475

9.5.1.2 TDD 1476

9.5.2 Minimum requirement (CSI Reference Symbols) 1477

9.5.2.1 FDD 1477

9.5.2.2 TDD 1479

9.5.3 Minimum requirement (CSI measurements in case two CSI subframe sets are configured) 1481

9.5.3.1 FDD 1481

9.5.3.2 TDD 1484

9.5.4 Minimum requirement (CSI measurements in case two CSI subframe sets are configured and CRS assistance information are configured) 1487

9.5.4.1 FDD 1487

9.5.4.2 TDD 1490

9.5.5 Minimum requirement (with CSI process) 1493

9.5.5.1 FDD 1494

9.5.5.2 TDD 1497

9.6 Additional requirements for carrier aggregation 1500

9.6.1 Periodic reporting on multiple cells (Cell-Specific Reference Symbols) 1500

9.6.1.1 FDD 1500

9.6.1.2 TDD 1506

9.6.1.3 TDD-FDD CA with FDD PCell 1512

9.6.1.4 TDD-FDD CA with TDD PCell 1517

9.7 CSI reporting (Single receiver antenna) 1523

9.7.1 CQI reporting definition under AWGN conditions 1524

9.7.1.1 FDD and half-duplex FDD 1524

9.7.1.2 TDD 1524

9.7.1.3 FDD (Category 1bis UE) 1525

9.7.1.4 TDD (Category 1bis UE) 1526

9.7.2 CQI reporting under fading conditions 1527

9.7.2.1 FDD and half-duplex FDD 1527

9.7.2.2 TDD 1528

9.7.2.3 FDD (Category 1bis UE) 1529

9.7.2.4 TDD (Category 1bis UE) 1530

9.8 CSI reporting (UE supporting coverage enhancement) 1531

9.8.1 CQI reporting definition under AWGN conditions 1531

9.8.1.1 FDD and half-duplex FDD 1531

9.8.1.2 TDD 1532

9.8.2 UE-selected subband CQI 1533

9.8.2.1 FDD and half-duplex FDD 1533

9.8.2.2 TDD 1537

9.8.3 CQI reporting definition for UE supporting 64QAM under AWGN 1540

9.8.3.1 FDD and half-duplex FDD 1540

9.8.3.2 TDD 1541

9.8.4 CQI reporting definition for UE supporting alternative table under AWGN 1542

9.8.4.1 FDD and half-duplex FDD 1542

9.8.4.2 TDD 1543

9.8.5 PMI reporting with PUCCH 1-1 (CSI Reference Symbol) 1544

9.8.5.1 FDD 1545

9.8.5.2 TDD 1546

9.9 CSI reporting for 4Rx UE 1547

9.9.1 CQI reporting definition under AWGN conditions 1547

9.9.1.1 Minimum requirement PUCCH 1-0 with Rank 1 (Cell-Specific Reference Symbols) 1548

9.9.1.1.1 FDD 1548

9.9.1.1.2 TDD 1548

9.9.1.2 Minimum requirement PUCCH 1-1 with Rank 2 (CSI Reference Symbols) 1549

9.9.1.2.1 FDD 1549

9.9.1.2.2 TDD 1550

9.9.1.3 Minimum requirement PUCCH 1-1 with Rank 4 (Cell-Specific Reference Symbols) 1551

9.9.1.3.1 FDD 1552

9.9.1.3.2 TDD 1552

9.9.1.4 Minimum requirement PUCCH 1-1 with Rank 3 (CSI Reference Symbols) 1553

9.9.1.4.1 FDD 1553

9.9.1.4.2 TDD 1554

9.9.2 CQI reporting definition under fading conditions 1555

9.9.2.1 Minimum requirement PUCCH 1-0 (Cell-Specific Reference Symbol) for enhanced receiver Type A 1555

9.9.2.1.1 FDD 1556

9.9.2.1.2 TDD 1557

9.9.2.2 Minimum requirement PUCCH 1-1 (CSI Reference Symbol) for enhanced receiver Type A 1559

9.9.2.2.1 FDD 1559

9.9.2.2.2 TDD 1562

9.9.3 Reporting of Precoding Matrix Indicator (PMI) for 4Rx UE 1565

9.9.3.1 Minimum requirement PUSCH 3-1 (CSI Reference Symbol) 1566

9.9.3.1.1 TDD 1566

9.9.4 Reporting of Rank Indicator (RI) 1568

9.9.4.1 Minimum requirement (Cell-Specific Reference Symbols) 1568

9.9.4.1.1 FDD 1568

9.9.4.1.2 TDD 1570

9.9.4.2 Minimum requirement (CSI Reference Symbols) 1571

9.9.4.2.1 FDD 1571

9.9.4.2.2 TDD 1573

9.10 Reporting of CSI-RS Resource Indicator (CRI) 1575

9.10.1 Minimum requirement (PUSCH 3-1) 1576

9.10.1.1 FDD 1576

9.10.1.2 TDD 1578

9.10.2 Minimum requirement (PUSCH 3-1, QCL Type C) 1580

9.10.2.1 FDD 1580

9.10.2.2 TDD 1583

9.11 Reporting of Hybrid Channel state information 1586

9.11.1 Minimum requirement (with eMIMO-Type configured as Class B with more than one CSI-RS resource configured and eMIMO-Type2 as Class B with one CSI-RS resource configured) 1586

9.11.1.1 FDD 1587

9.11.1.2 TDD 1589

9.12 CSI reporting (UE supporting Short TTI) 1591

9.12.1 CQI reporting under fading conditions (Cell-Specific Reference Symbol) 1591

9.12.1.1 FDD 1591

9.12.1.2 TDD 1594

9.12.2 CQI reporting under fading conditions (CSI Reference Symbol) 1595

9.12.2.1 FDD 1595

9.12.2.2 TDD 1598

9.13 CSI reporting for 8Rx UE 1600

9.13.1 CQI reporting definition under AWGN conditions 1600

9.13.1.1 Minimum requirement PUCCH 1-1 with Rank 4 (CSI Reference Symbols) 1600

9.13.1.2.1 Void 1600

9.13.1.2.2 TDD 1600

9.14 CSI reporting of Narrowband IoT 1601

9.14.1 CQI reporting definition under AWGN conditions 1601

9.14.1.1 Half-duplex FDD 1601

9.14.1.2 TDD 1602

10 Performance requirement (MBMS) 1603

10.1 FDD (Fixed Reference Channel) 1603

10.1.1 Minimum requirement 1604

10.2 TDD (Fixed Reference Channel) 1605

10.2.1 Minimum requirement 1605

10.3 FDD (Fixed Reference Channel) with FeMBMS 1606

10.3.1 Minimum requirement for FeMBMS Unicast-mixed Cell under CA 1606

10.3.1.1 Minimum requirement with 1.25kHz subcarrier spacing 1606

10.3.1.2 Minimum requirement with 7.5kHz subcarrier spacing 1607

10.3.2 Minimum requirement for FeMBMS Unicast-mixed Cell as Non-Serving Cell 1608

10.3.2.1 Minimum requirement with 1.25kHz subcarrier spacing 1608

10.3.2.2 Minimum requirement with 7.5kHz subcarrier spacing 1609

10.3.3 Minimum requirement for MBMS Dedicated cell 1610

10.3.3.1 Minimum requirement with 1.25kHz subcarrier spacing 1610

10.3.3.2 Minimum requirement with 7.5kHz subcarrier spacing 1611

10.3.3.3 Minimum requirement with 15kHz subcarrier spacing 1612

10.4 FDD with 5G terrestrial broadcast 1613

10.4.1 Minimum requirement for PMCH decoding 1613

10.4.1.1 Minimum requirement with 0.37kHz subcarrier spacing 1613

10.4.1.2 Minimum requirement with 2.5kHz subcarrier spacing 1614

10.4.2 Minimum requirement for CAS detection 1615

10.4.2.1 Minimum requirement for PBCH detection 1615

11 Performance requirement (ProSe Direct Discovery) 1615

11.1 General 1616

11.1.1 Applicability of requirements 1616

11.1.2 Reference DRX configuration 1616

11.2 Demodulation of PSDCH (single link performance) 1616

11.2.1 FDD (in-coverage) 1616

11.2.2 TDD (in-coverage) 1617

11.2.3 FDD (out-of-coverage) 1618

11.3 Power imbalance performance with two links 1619

11.3.1 FDD 1619

11.3.2 TDD 1620

11.4 Multiple timing reference test 1621

11.4.1 FDD 1622

11.5 Maximum Sidelink processes test 1623

11.5.1 FDD 1623

11.5.2 TDD 1624

12 Performance requirement (ProSe Direct Communication) 1626

12.1 General 1626

12.1.1 Applicability of requirements 1626

12.1.1.1 Applicability of requirements for different channel bandwidths 1626

12.1.1.2 Test coverage for different number of component carriers 1626

12.1.1.3 Applicability and test rules for different CA configurations and bandwidth combination sets 1626

12.1.2 Reference DRX configuration 1627

12.2 Demodulation of PSSCH 1627

12.2.1 FDD 1627

12.3 Demodulation of PSCCH 1628

12.3.1 FDD 1629

12.4 Demodulation of PSBCH 1630

12.4.1 FDD 1630

12.5 Power imbalance performance with two links 1630

12.5.1 FDD 1630

12.6 Multiple timing reference test 1632

12.6.1 FDD 1632

12.7 Maximum Sidelink processes test 1635

12.7.1 FDD 1635

12.8 Sustained downlink data rate with active Sidelink 1636

13 Void 1638

14 Performance requirement (V2X Sidelink Communication) 1638

14.1 General 1638

14.1.1 Applicability of requirements 1638

14.2 Demodulation of PSSCH 1639

14.3 Demodulation of PSCCH 1640

14.4 Power imbalance performance with two links 1640

14.5 Demodulation of PSBCH 1641

14.6 Demodulation of PSSCH with eNB based synchronization 1642

14.7 Soft buffer test 1642

14.8 PSCCH/PSSCH decoding capability test 1643

14.9 Sustained downlink data rate with active sidelink 1644

14.10 Soft buffer test (CA) 1645

14.11 PSCCH/PSSCH decoding capability test (CA) 1646

Annex A (normative): Measurement channels 1646

A.1 General 1646

A.2 UL reference measurement channels 1646

A.2.1 General 1646

A.2.1.1 Applicability and common parameters 1646

A.2.1.2 Determination of payload size 1646

A.2.1.3 Overview of UL reference measurement channels 1647

A.2.2 Reference measurement channels for FDD 1670

A.2.2.1 Full RB allocation 1670

A.2.2.1.1 QPSK 1670

A.2.2.1.2 16-QAM 1672

A.2.2.1.3 64-QAM 1674

A.2.2.1.4 256 QAM 1675

A.2.2.2 Partial RB allocation 1675

A.2.2.2.1 QPSK 1676

A.2.2.2.2 16-QAM 1679

A.2.2.2.3 64-QAM 1681

A.2.2.2.4 256 QAM 1683

A.2.2.3 Void 1683

A.2.2.4 subPRB allocation 1684

A.2.3 Reference measurement channels for TDD 1684

A.2.3.1 Full RB allocation 1684

A.2.3.1.1 QPSK 1684

A.2.3.1.2 16-QAM 1687

A.2.3.1.3 64-QAM 1689

A.2.3.1.4 256 QAM 1690

A.2.3.2 Partial RB allocation 1690

A.2.3.2.1 QPSK 1691

A.2.3.2.2 16-QAM 1695

A.2.3.2.3 64-QAM 1700

A.2.3.2.4 256 QAM 1702

A.2.3.3 Void 1702

A.2.3.4 subPRB allocation 1703

A.2.4 Reference measurement channels for UE category NB1 1703

A.2.5 Reference measurement channels for LAA 1704

A.2.5.1 Full RB allocation 1704

A.2.5.1.1 QPSK 1704

A.2.5.1.2 16QAM 1705

A.2.5.1.3 64QAM 1705

A.2.5.2 Partial RB allocation 1705

A.2.5.2.1 QPSK 1706

A.2.5.2.2 16QAM 1706

A.2.5.2.3 64QAM 1707

A.3 DL reference measurement channels 1707

A.3.1 General 1707

A.3.1.1 Overview of DL reference measurement channels 1708

A.3.2 Reference measurement channel for receiver characteristics 1733

A.3.3 Reference measurement channels for PDSCH performance requirements (FDD) 1763

A.3.3.1 Single-antenna transmission (Common Reference Symbols) 1763

A.3.3.2 Multi-antenna transmission (Common Reference Symbols) 1768

A.3.3.2.1 Two antenna ports 1768

A.3.3.2.2 Four antenna ports 1777

A.3.3.3 Reference Measurement Channel for UE-Specific Reference Symbols 1782

A.3.3.3.0 Two antenna ports (no CSI-RS) 1782

A.3.3.3.1 Two antenna port (CSI-RS) 1783

A.3.3.3.2 Four antenna ports (CSI-RS) 1786

A.3.3.3.2A Eight antenna ports (CSI-RS) 1793

A.3.3.3.3 Twelve antenna port (CSI-RS) 1795

A.3.3.3.4 Sixteen antenna port (CSI-RS) 1796

A.3.3.3.5 Twenty-four antenna port (CSI-RS) 1797

A.3.3.3.6 Thirty-two antenna port (CSI-RS) 1798

A.3.4 Reference measurement channels for PDSCH performance requirements (TDD) 1800

A.3.4.1 Single-antenna transmission (Common Reference Symbols) 1800

A.3.4.2 Multi-antenna transmission (Common Reference Signals) 1808

A.3.4.2.1 Two antenna ports 1808

A.3.4.2.2 Four antenna ports 1821

A.3.4.3 Reference Measurement Channels for UE-Specific Reference Symbols 1828

A.3.4.3.1 Single antenna port (Cell Specific) 1828

A.3.4.3.2 Two antenna ports (Cell Specific) 1829

A.3.4.3.3 Two antenna ports (CSI-RS) 1831

A.3.4.3.4 Four antenna ports (CSI-RS) 1839

A.3.4.3.5 Eight antenna ports (CSI-RS) 1846

A.3.4.3.6 Twelve antenna ports (CSI-RS) 1852

A.3.4.3.7 Sixteen antenna ports (CSI-RS) 1853

A.3.4.3.8 Twenty-four antenna ports (CSI-RS) 1854

A.3.4.3.9 Thirty-two antenna ports (CSI-RS) 1855

A.3.5 Reference measurement channels for PDCCH/PCFICH performance requirements 1857

A.3.5.1 FDD 1857

A.3.5.2 TDD 1857

A.3.5.3 LAA 1858

A.3.6 Reference measurement channels for PHICH performance requirements 1858

A.3.7 Reference measurement channels for PBCH performance requirements 1858

A.3.8 Reference measurement channels for MBMS performance requirements 1859

A.3.8.1 FDD 1859

A.3.8.2 TDD 1864

A.3.9 Reference measurement channels for sustained downlink data rate provided by lower layers 1866

A.3.9.1 FDD 1866

A.3.9.2 TDD 1870

A.3.9.3 FDD (EPDCCH scheduling) 1884

A.3.9.4 TDD (EPDCCH scheduling) 1885

A.3.9.5 LAA 1887

A.3.10 Reference Measurement Channels for EPDCCH performance requirements 1889

A.3.10.1 FDD 1889

A.3.10.2 TDD 1889

A.3.11 Reference Measurement Channels for MPDCCH performance requirements 1889

A.3.11.1 FDD and half-duplex FDD 1889

A.3.11.2 TDD 1890

A.3.12 Reference measurement channels for NPDSCH performance requirements 1891

A.3.12.1 In-band 1891

A.3.12.1.2 Two-antenna transmission 1891

A.3.12.2 Standalone/Guard-band 1893

A.3.12.2.1 Single-antenna transmission 1893

A.3.13 Reference measurement channels for NPDCCH performance requirements 1896

A.3.13.1 Half-duplex FDD 1896

A.3.13.2 TDD 1897

A.3.14 Reference measurement channels for NPBCH performance requirements for Cat NB1 UEs 1897

A.3.15 Reference Measurement Channels for LAA SCell with frame structure Type-3 1898

A.3.15.1 Multi-antenna transmission (Common Reference Symbols) 1898

A.3.15.1.1 Four antenna ports 1898

A.3.15.2 Reference Measurement Channel for UE-Specific Reference Symbols 1898

A.3.15.2.1 Two antenna ports (CSI-RS) 1898

A.3.16 Reference measurement channels for Slot-PDSCH and Subslot-PDSCH performance requirements 1900

A.3.16.1 FDD 1900

A.3.16.2 TDD 1904

A.3.17 Reference measurement channels for SPDCCH performance requirements 1905

A.3.17.1 FDD 1905

A.3.17.2 TDD 1906

A.4 CSI reference measurement channels 1906

A.5 OFDMA Channel Noise Generator (OCNG) 1921

A.5.1 OCNG Patterns for FDD 1921

A.5.1.1 OCNG FDD pattern 1: One sided dynamic OCNG FDD pattern 1921

A.5.1.2 OCNG FDD pattern 2: Two sided dynamic OCNG FDD pattern 1922

A.5.1.3 OCNG FDD pattern 3: 49 RB OCNG allocation with MBSFN in 10 MHz 1922

A.5.1.3A OCNG FDD pattern 3A: 49 RB OCNG allocation with MBSFN enhancement in 10 MHz 1923

A.5.1.4 OCNG FDD pattern 4: One sided dynamic OCNG FDD pattern for MBMS transmission 1923

A.5.1.4A OCNG FDD pattern 4A: One sided dynamic OCNG FDD pattern for enhanced MBMS transmission 1924

A.5.1.5 OCNG FDD pattern 5: One sided dynamic 16QAM modulated OCNG FDD pattern 1925

A.5.1.6 OCNG FDD pattern 6: dynamic OCNG FDD pattern when user data is in 2 non-contiguous blocks 1926

A.5.1.8 OCNG FDD pattern 8: Dynamic OCNG FDD pattern for TM10 transmission 1927

A.5.2 OCNG Patterns for TDD 1928

A.5.2.1 OCNG TDD pattern 1: One sided dynamic OCNG TDD pattern 1928

A.5.2.2 OCNG TDD pattern 2: Two sided dynamic OCNG TDD pattern 1929

A.5.2.3 OCNG TDD pattern 3: 49 RB OCNG allocation with MBSFN in 10 MHz 1930

A.5.2.4 OCNG TDD pattern 4: One sided dynamic OCNG TDD pattern for MBMS transmission 1930

A.5.2.5 OCNG TDD pattern 5: One sided dynamic 16QAM modulated OCNG TDD pattern 1931

A.5.2.6 OCNG TDD pattern 6: dynamic OCNG TDD pattern when user data is in 2 non-contiguous blocks 1932

A.5.2.8 OCNG TDD pattern 8: Dynamic OCNG TDD pattern for TM10 transmission 1933

A.5.3 OCNG Patterns for Narrowband IoT 1934

A.5.3.1 Narrowband IoT OCNG pattern 1 1934

A.5.4 OCNG Patterns for frame structure type 3 1935

A.5.4.1 OCNG FS3 pattern 1: One sided dynamic OCNG frame structure type 3 pattern 1935

A.5.4.2 OCNG FS3 pattern 2: Two sided dynamic OCNG frame structure 3 pattern 1936

A.6 Sidelink reference measurement channels 1937

A.6.1 General 1937

A.6.1.1 Overview of ProSe reference measurement channels 1937

A.6.2 Reference measurement channel for receiver characteristics 1938

A.6.3 Reference measurement channels for PSDCH performance requirements 1940

A.6.4 Reference measurement channels for PSCCH performance requirements 1941

A.6.5 Reference measurement channels for PSSCH performance requirements 1941

A.6.6 Reference measurement channels for PSBCH performance requirements 1942

A.7 Sidelink reference resource pool configurations 1943

A.7.1 Reference resource pool configurations for ProSe Direct Discovery demodulation tests 1943

A.7.1.1 FDD 1943

A.7.1.2 TDD 1946

A.7.2 Reference resource pool configurations for ProSe Direct Communication demodulation tests 1948

A.7.2.1 FDD 1948

A.8 V2X reference measurement channels 1953

A.8.1 General 1953

A.8.1.1 Overview of V2X reference measurement channels 1954

A.8.2 Reference measurement channel for receiver characteristics 1954

A.8.3 Reference measurement channel for transmitter characteristics 1956

A.8.4 Reference measurement for PSCCH performance requirements 1959

A.8.5 Reference measurement for PSSCH performance requirements 1960

A.8.6 Reference measurement for PSBCH performance requirements 1960

A.9 V2X reference resource pool configurations 1961

Annex B (normative): Propagation conditions 1964

B.1 Static propagation condition 1964

B.1.1 UE Receiver with 2Rx 1964

B.1.2 UE Receiver with 4Rx 1964

B.1.3 UE Receiver with 8Rx 1965

B.2 Multi-path fading propagation conditions 1966

B.2.1 Delay profiles 1966

B.2.2 Combinations of channel model parameters 1967

B.2.3 MIMO Channel Correlation Matrices 1968

B.2.3.1 Definition of MIMO Correlation Matrices 1968

B.2.3.2 MIMO Correlation Matrices at High, Medium and Low Level 1974

B.2.3A MIMO Channel Correlation Matrices using cross polarized antennas 1977

B.2.3A.1 Definition of MIMO Correlation Matrices using cross polarized antennas 1978

B.2.3A.2 Spatial Correlation Matrices using cross polarized antennas at eNB and UE sides 1978

B.2.3A.2.1 Spatial Correlation Matrices at eNB side 1978

B.2.3A.2.2 Spatial Correlation Matrices at UE side 1979

B.2.3A.4 Beam steering approach 1982

B.2.3B MIMO Channel Correlation Matrices using two-dimension cross polarized antennas at eNB and cross polarized antennas at UE 1982

B.2.3B.1 Definition of MIMO Correlation Matrices using two-dimension cross polarized antennas at eNB and cross polarized antennas at UE 1983

B.2.3B.2 Spatial Correlation Matrices using two-dimension cross polarized antennas at eNB and cross polarized antennas at UE 1984

B.2.3B.2.1 Spatial Correlation Matrices at eNB side 1984

B.2.3B.2.2 Spatial Correlation Matrices at UE side 1984

B.2.3B.3 MIMO Correlation Matrices using two-dimension cross polarized antennas at eNB and cross polarized antennas at UE 1984

B.2.3B.4 Beam steering approach 1987

B.2.3B.4A Beam steering approach with dual cluster beams 1988

B.2.4 Propagation conditions for CQI tests 1989

B.2.4.1 Propagation conditions for CQI tests with multiple CSI processes 1989

B.2.5 Void 1989

B.2.6 MBSFN Propagation Channel Profile 1989

B.2.6.1 Subcarrier spacing 15kHz or 7.5kHz 1989

B.2.6.2 Subcarrier spacing 1.25kHz 1990

B.2.6.3 Subcarrier spacing 0.37kHz 1991

B.2.6.4 Subcarrier spacing 2.5kHz 1991

B.3 High speed train scenario 1992

B.3A HST-SFN scenario 1993

B.3B HST-SFN scenario for 500 km/h speed 1997

B.3C HST scenario for 500 km/h speed 1997

B.4 Beamforming Model 1997

B.4.1 Single-layer random beamforming (Antenna port 5, 7, or 8) 1997

B.4.1A Single-layer random beamforming (Antenna port 7, 8, 11 or 13 with enhanced DMRS table configured) 1998

B.4.2 Dual-layer random beamforming (antenna ports 7 and 8) 1998

B.4.3 Generic beamforming model (antenna ports 7-14) 1999

B.4.4 Random beamforming for EPDCCH distributed transmission (Antenna port 107 and 109) 1999

B.4.5 Random beamforming for EPDCCH localized transmission (Antenna port 107, 108, 109 or 110) 2000

B.4.6 Beamforming model for CRI test 2000

B.5 Interference models for enhanced performance requirements Type-A 2001

B.5.1 Dominant interferer proportion 2002

B.5.2 Transmission mode 3 interference model 2002

B.5.3 Transmission mode 4 interference model 2002

B.5.4 Transmission mode 9 interference model 2003

B.6 Interference models for enhanced performance requirements Type-B 2003

B.6.1 Transmission mode 2 interference model 2003

B.6.2 Transmission mode 3 interference model 2003

B.6.3 Transmission mode 4 interference model 2004

B.6.4 Transmission mode 9 interference model 2004

B.6.5 CRS interference model 2005

B.6.6 Random interference model 2005

B.7 Interference models for enhanced downlink control channel performance requirements Type A and B 2006

B.7.1 PDCCH, PCFICH and PHICH interference model 2006

B.8 Burst transmission models for Frame structure type 3 2007

B.8.1 Burst transmission model for one LAA SCell 2007

B.8.2 Burst transmission model for multiple LAA SCell(s) 2007

Annex C (normative): Downlink Physical Channels 2009

C.1 General 2009

C.2 Set-up 2009

C.3 Connection 2009

C.3.1 Measurement of Receiver Characteristics 2009

C.3.2 Measurement of Performance requirements 2010

C.3.3 Aggressor cell power allocation for Measurement of Performance Requirements when ABS is Configured 2011

C.3.4 Power Allocation for Measurement of Performance Requirements when Quasi Co-location Type B: same Cell ID 2012

C.3.5 Simplified CA testing method 2012

C.3.6 Measurement of Receiver Characteristics for Narrowband IoT 2013

Annex D (normative): Characteristics of the interfering signal 2014

D.1 General 2014

D.2 Interference signals 2014

Annex E (normative): Environmental conditions 2015

E.1 General 2015

E.2 Environmental 2015

E.2.1 Temperature 2015

E.2.2 Voltage 2015

E.2.3 Vibration 2016

Annex F (normative): Transmit modulation 2017

F.1 Measurement Point 2017

F.2 Basic Error Vector Magnitude measurement 2017

F.3 Basic in-band emissions measurement 2018

F.4 Modified signal under test 2018

F.5 Window length 2020

F.5.1 Timing offset 2020

F.5.2 Window length 2020

F.5.3 Window length for normal CP 2020

F.5.4 Window length for Extended CP 2021

F.5.5 Window length for PRACH 2021

F.5.F Window length for category NB1 2022

F.6 Averaged EVM 2022

F.6.F Averaged EVM for category NB1 2023

F.7 Spectrum Flatness 2023

Annex G (informative): Reference sensitivity level in lower SNR 2024

G.1 General 2024

G.2 Typical receiver sensitivity performance (QPSK) 2024

G.3 Reference measurement channel for REFSENSE in lower SNR 2030

Annex H (normative): Modified MPR behavior 2033

H.1 Indication of modified MPR behavior 2033

Annex I (normative): Supported Post Antenna Gain 2034

I.1 Declared Supported Post Antenna Gain for UE 2034

Annex J (informative): Change history 2035