|  |  |
| --- | --- |
| 3GPP TS 36.101 V16.15.0 (2022-09) | |
| Technical Specification | |
| 3rd Generation Partnership Project;  Technical Specification Group Radio Access Network;  Evolved Universal Terrestrial Radio Access (E-UTRA);  User Equipment (UE) radio transmission and reception  (Release 16) | |
|  | |
| *LTE-AdvancedPro_largerTM_cropped* | 3GPP-logo_web |
|  | |
| The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP. The present document has not been subject to any approval process by the 3GPPOrganizational Partners and shall not be implemented. This Specification is provided for future development work within 3GPPonly. The Organizational Partners accept no liability for any use of this Specification. Specifications and Reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organizational Partners' Publications Offices. | |

|  |
| --- |
|  |
| ***3GPP***  Postal address  3GPP support office address  650 Route des Lucioles - Sophia Antipolis  Valbonne - FRANCE  Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16  Internet  http://www.3gpp.org |
| ***Copyright Notification***  No part may be reproduced except as authorized by written permission. The copyright and the foregoing restriction extend to reproduction in all media.  © 2022, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).  All rights reserved.  UMTS™ is a Trade Mark of ETSI registered for the benefit of its members  3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  GSM® and the GSM logo are registered and owned by the GSM Association |

Contents

Foreword 32

1 Scope 34

2 References 34

3 Definitions, symbols and abbreviations 34

3.1 Definitions 34

3.2 Symbols 36

3.3 Abbreviations 39

4 General 41

4.1 Relationship between minimum requirements and test requirements 41

4.2 Applicability of minimum requirements 41

4.3 Void 41

4.3A Applicability of minimum requirements (CA, UL-MIMO, ProSe, Dual Connectivity, UE category 0, UE category M1, UE category M2, UE category 1bis, UE category NB1 and NB2, V2X Communication, MBMS UE) 41

4.4 RF requirements in later releases 43

5 Operating bands and channel arrangement 43

5.1 General 43

5.2 Void 43

5.3 Void 43

5.4 Void 43

5.5 Operating bands 43

5.5A Operating bands for CA 46

5.5B Operating bands for UL-MIMO 65

5.5C Operating bands for Dual Connectivity 65

5.5D Operating bands for ProSe 68

5.5E Operating bands for UE category 0, UE category M1 and M2 and UE category 1bis 69

5.5F Operating bands for category NB1 and NB2 69

5.5G Operating bands for V2X Communication 69

5.6 Channel bandwidth 70

5.6.1 Channel bandwidths per operating band 71

5.6A Channel bandwidth for CA 74

5.6A.1 Channel bandwidths per operating band for CA 76

5.6B Channel bandwidth for UL-MIMO 178

5.6B.1 Void 178

5.6C Channel bandwidth for Dual Connectivity 178

5.6C.1 Void 178

5.6D Channel bandwidth for ProSe 178

5.6D.1 Channel bandwidths per operating band for ProSe 178

5.6F Channel bandwidth for category NB1 and NB2 179

5.6G Channel bandwidth for V2X Communication 180

5.6G.1 Channel bandwidths per operating band for V2X Communication 180

5.7 Channel arrangement 182

5.7.1 Channel spacing 182

5.7.1A Channel spacing for CA 182

5.7.1F Channel spacing for category NB1 and NB2 183

5.7.2 Channel raster 183

5.7.2A Channel raster for CA 183

5.7.2F Channel raster for category NB1 and NB2 183

5.7.3 Carrier frequency and EARFCN 183

5.7.3F Carrier frequency and EARFCN for category NB1 and NB2 186

5.7.4 TX–RX frequency separation 186

5.7.4A TX–RX frequency separation for CA 187

5.7.4E TX–RX frequency separation for category M1 and M2 187

5.7.4F TX–RX frequency separation for category NB1 and NB2 188

6 Transmitter characteristics 188

6.1 General 188

6.2 Transmit power 188

6.2.1 Void 188

6.2.2 UE maximum output power 188

6.2.2A UE maximum output power for CA 191

6.2.2B UE maximum output power for UL-MIMO 196

6.2.2C Void 199

6.2.2D UE maximum output power for ProSe 199

6.2.2E UE maximum output power for Category M1 and M2 UE 199

6.2.2F UE maximum output power for category NB1 and NB2 200

6.2.2G UE maximum output power for V2X Communication 201

6.2.3 UE maximum output power for modulation / channel bandwidth 203

6.2.3A UE Maximum Output power for modulation / channel bandwidth for CA 204

6.2.3B UE maximum output power for modulation / channel bandwidth for UL-MIMO 209

6.2.3D UE maximum output power for modulation / channel bandwidth for ProSe 209

6.2.3E UE maximum output power for modulation / channel bandwidth for category M1 and M2 210

6.2.3F UE maximum output power for modulation / channel bandwidth for category NB1 and NB2 212

6.2.3G UE maximum output power for modulation / channel bandwidth for V2X Communication 212

6.2.3G.1 MPR for Power class 3 V2X UE 212

6.2.3G.2 MPR for Power class 2 V2X UE 214

6.2.4 UE maximum output power with additional requirements 214

6.2.4A UE maximum output power with additional requirements for CA 233

6.2.4A.1 A-MPR for CA\_NS\_01 for CA\_1C 235

6.2.4A.2 A-MPR for CA\_NS\_02 for CA\_1C 236

6.2.4A.3 A-MPR for CA\_NS\_03 for CA\_1C 236

6.2.4A.4 A-MPR for CA\_NS\_04 237

6.2.4A.5 A-MPR for CA\_NS\_05 for CA\_38C 240

6.2.4A.6 A-MPR for CA\_NS\_06 241

6.2.4A.7 A-MPR for CA\_NS\_07 242

6.2.4A.8 A-MPR for CA\_NS\_08 243

6.2.4A.9 Void 244

6.2.4A.10 A-MPR for CA\_NS\_10 244

6.2.4B UE maximum output power with additional requirements for UL-MIMO 249

6.2.4D UE maximum output power with additional requirements for ProSe 249

6.2.4E UE maximum output power with additional requirements for category M1 and M2 UE 249

6.2.4F UE maximum output power with additional requirements for category NB1 and NB2 UE 258

6.2.4G UE maximum output power with additional requirements for V2X Communication 259

6.2.5 Configured transmitted power 261

6.2.5A Configured transmitted power for CA 292

6.2.5B Configured transmitted power for UL-MIMO 296

6.2.5C Configured transmitted power for Dual Connectivity 296

6.2.5D Configured transmitted power for ProSe 298

6.2.5F Configured transmitted Power for category NB1 and NB2 299

6.2.5G Configured transmitted power for V2X Communication 300

6.3 Output power dynamics 304

6.3.1 (Void) 304

6.3.2 Minimum output power 304

6.3.2.1 Minimum requirement 304

6.3.2A UE Minimum output power for CA 304

6.3.2A.1 Minimum requirement for CA 305

6.3.2B UE Minimum output power for UL-MIMO 305

6.3.2B.1 Minimum requirement 305

6.3.2C Void 305

6.3.2D UE Minimum output power for ProSe 305

6.3.2F UE Minimum output power for category NB1 and NB2 306

6.3.2G UE Minimum output power for V2X Communication 306

6.3.3 Transmit OFF power 306

6.3.3.1. Minimum requirement 306

6.3.3A UE Transmit OFF power for CA 307

6.3.3A.1 Minimum requirement for CA 307

6.3.3B UE Transmit OFF power for UL-MIMO 307

6.3.3B.1 Minimum requirement 307

6.3.3D Transmit OFF power for ProSe 308

6.3.3F Transmit OFF power for category NB1 and NB2 308

6.3.3G Transmit OFF power for V2X Communication 308

6.3.4 ON/OFF time mask 309

6.3.4.1 General ON/OFF time mask 309

6.3.4.2 PRACH and SRS time mask 310

6.3.4.2.1 PRACH time mask 310

6.3.4.2.2 SRS time mask 311

6.3.4.3 Slot / Sub frame boundary time mask for subframe TTI 313

6.3.4.4 PUCCH / PUSCH / SRS time mask for subframe TTI 315

6.3.4.5 Symbol / Subslot boundary time mask for subslot TTI 317

6.3.4.6 Subslot PUCCH / subslot PUSCH / SRS time mask for subslot TTI 318

6.3.4.7 Symbol / Slot boundary time mask for slot TTI 321

6.3.4.8 Slot PUCCH / slot PUSCH / SRS time mask for slot TTI 322

6.3.4.9 Consecutive subslot and slot TTI or consecutive subslot and subframe TTI time mask 322

6.3.4.10 Consecutive subframe and subslot TTI or consecutive slot and subslot TTI time mask 322

6.3.4.11 Consecutive TTI and slot TTI or consecutive slot TTI and TTI time mask 323

6.3.4A ON/OFF time mask for CA 324

6.3.4B ON/OFF time mask for UL-MIMO 324

6.3.4D ON/OFF time mask for ProSe 324

6.3.4D.1 General time mask for ProSe 324

6.3.4D.2 PSSS/SSSS time mask 325

6.3.4D.3 PSSS / SSSS / PSBCH time mask 326

6.3.4D.4 PSSCH / SRS time mask 326

6.3.4F ON/OFF time mask for category NB1 and NB2 326

6.3.4F.1 General ON/OFF time mask 326

6.3.4F.2 NPRACH time mask 327

6.3.4G ON/OFF time mask for V2X Communication 327

6.3.4G.1 PSSS / SSSS / PSBCH time mask 328

6.3.5 Power Control 328

6.3.5.1 Absolute power tolerance 328

6.3.5.1.1 Minimum requirements 328

6.3.5.2 Relative Power tolerance 329

6.3.5.2.1 Minimum requirements 329

6.3.5.3 Aggregate power control tolerance 330

6.3.5.3.1 Minimum requirement 330

6.3.5A Power control for CA 330

6.3.5A.1 Absolute power tolerance 330

6.3.5A.1.1 Minimum requirements 330

6.3.5A.2 Relative power tolerance 331

6.3.5A.2.1 Minimum requirements 331

6.3.5A.3 Aggregate power control tolerance 331

6.3.5A.3.1 Minimum requirements 331

6.3.5B Power control for UL-MIMO 332

6.3.5D Power Control for ProSe 332

6.3.5D.1 Absolute power tolerance 332

6.3.5E Power control for category M1 and M2 332

6.3.5E.1 Absolute power tolerance 332

6.3.5E.2 Relative Power tolerance 332

6.3.5E.3 Aggregate power control tolerance 333

6.3.5E.3.1 Minimum requirement 333

6.3.5F Power Control for category NB1 and NB2 333

6.3.5F.1 Absolute power tolerance 334

6.3.5F.2 Relative power tolerance 334

6.3.5F.3 Aggregate power control tolerance for category NB1 and NB2 335

6.3.5F.3.1 Minimum requirement 335

6.3.5G Power Control for V2X Communication 335

6.3.5G.1 Absolute power tolerance 335

6.4 Void 336

6.5 Transmit signal quality 336

6.5.1 Frequency error 336

6.5.1A Frequency error for CA 336

6.5.1B Frequency error for UL-MIMO 336

6.5.1D Frequency error for ProSe 336

6.5.1E Frequency error for UE category M1 and M2 336

6.5.1F Frequency error for UE category NB1 and NB2 337

6.5.1G Frequency error for V2X Communication 337

6.5.2 Transmit modulation quality 337

6.5.2.1 Error Vector Magnitude 338

6.5.2.1.1 Minimum requirement 338

6.5.2.2 Carrier leakage 338

6.5.2.2.1 Minimum requirements 339

6.5.2.3 In-band emissions 339

6.5.2.3.1 Minimum requirements 339

6.5.2.4 EVM equalizer spectrum flatness 340

6.5.2.4.1 Minimum requirements 340

6.5.2A Transmit modulation quality for CA 341

6.5.2A.1 Error Vector Magnitude 342

6.5.2A.2 Carrier leakage for CA 342

6.5.2A.2.1 Minimum requirements 342

6.5.2A.3 In-band emissions 342

6.5.2A.3.1 Minimum requirement for CA 342

6.5.2B Transmit modulation quality for UL-MIMO 345

6.5.2B.1 Error Vector Magnitude 345

6.5.2B.2 Carrier leakage 345

6.5.2B.3 In-band emissions 345

6.5.2B.4 EVM equalizer spectrum flatness for UL-MIMO 345

6.5.2D Transmit modulation quality for ProSe 345

6.5.2D.1 Error Vector Magnitude 345

6.5.2D.2 Carrier leakage 346

6.5.2D.3 In-band emissions 346

6.5.2D.4 EVM equalizer spectrum flatness for ProSe 346

6.5.2E Transmit modulation quality for category M1 and M2 346

6.5.2E.1 Error Vector Magnitude 346

The Error Vector Magnitude is defined in section 6.5.2.1. 346

6.5.2E.2 Carrier leakage 346

6.5.2E.2.1 Minimum requirements 346

6.5.2E.3 In-band emissions 346

6.5.2E.3.1 Minimum requirements 346

6.5.2F Transmit modulation quality for Category NB1 and NB2 348

6.5.2F.1 Error Vector Magnitude 348

6.5.2F.2 Carrier leakage 348

6.5.2F.3 In-band emissions 348

6.5.2G Transmit modulation quality for V2X Communication 349

6.5.2G.1 Error Vector Magnitude 349

6.5.2G.2 Carrier leakage 350

6.5.2G.3 In-band emissions 350

6.5.2G.4 EVM equalizer spectrum flatness 350

6.6 Output RF spectrum emissions 350

6.6.1 Occupied bandwidth 350

6.6.1.1 Additional minimum requirement for E-UTRA (network signalled value “NS\_29”) 351

6.6.1A Occupied bandwidth for CA 351

6.6.1B Occupied bandwidth for UL-MIMO 351

6.6.1F Occupied bandwidth for category NB1 and NB2 352

6.6.1G Occupied bandwidth for V2X Communication 352

6.6.2 Out of band emission 352

6.6.2.1 Spectrum emission mask 352

6.6.2.1.1 Minimum requirement 352

6.6.2.1A Spectrum emission mask for CA 353

6.6.2.2 Additional spectrum emission mask 354

6.6.2.2.1 Minimum requirement (network signalled value "NS\_03", “NS\_11”, "NS\_20", and “NS\_21”) 354

6.6.2.2.2 Minimum requirement (network signalled value "NS\_04") 355

6.6.2.2.3 Minimum requirement (network signalled value "NS\_06" or “NS\_07”) 355

6.6.2.2.4 Minimum requirement (network signalled value "NS\_33" or “NS\_34”) 356

6.6.2.2.5 Minimum requirement (network signalled value “NS\_27” and “NS\_43”) 356

6.6.2.2.6 Minimum requirement (network signalled value "NS\_28”) 357

6.6.2.2.7 Minimum requirement (network signalled value "NS\_35") 357

6.6.2.2A Additional Spectrum Emission Mask for CA 358

6.6.2.2A.1 Minimum requirement (network signalled value "CA\_NS\_04") 358

6.6.2.2A.2 Minimum requirement CA\_66B (network signalled value "CA\_NS\_09") 358

6.6.2.2A.3 Minimum requirement CA\_66C (network signalled value "CA\_NS\_09") 359

6.6.2.2A.4 Minimum requirement CA\_48B and CA\_48C (network signalled value "CA\_NS\_10") 359

6.6.2.3 Adjacent Channel Leakage Ratio 360

6.6.2.3.1 Minimum requirement E-UTRA 360

6.6.2.3.1a Additional minimum requirement for E-UTRA (network signalled value “NS\_29”) 361

6.6.2.3.1A Void 362

6.6.2.3.1Aa Void 362

6.6.2.3.2 Minimum requirements UTRA 362

6.6.2.3.2A Minimum requirement UTRA for CA 363

6.6.2.3.3A Minimum requirements for CA E-UTRA 365

6.6.2.4 Void 366

6.6.2.4.1 Void 366

6.6.2A Void 366

6.6.2B Out of band emission for UL-MIMO 366

6.6.2C Void 366

6.6.2D Out of band emission for ProSe 366

6.6.2F Out of band emission for category NB1 and NB2 367

6.6.2F.1 Spectrum emission mask 367

6.6.2F.2 Additional Spectrum Emission Mask for Category NB1 and NB2 367

6.6.2F.2.1 Minimum requirement (network signalled value "NS\_02") 367

6.6.2F.2.2 Minimum requirement (network signalled value "NS\_03") 367

6.6.2F.3 Adjacent Channel Leakage Ratio for category NB1 and NB2 368

6.6.2G Out of band emission for V2X Communication 368

6.6.3 Spurious emissions 369

6.6.3.1 Minimum requirements 369

6.6.3.1A Minimum requirements for CA 370

6.6.3.2 Spurious emission band UE co-existence 371

6.6.3.2A Spurious emission band UE co-existence for CA 380

6.6.3.3 Additional spurious emissions 395

6.6.3.3.1 Minimum requirement (network signalled value "NS\_05") 396

6.6.3.3.2 Minimum requirement (network signalled value “NS\_07”) 396

6.6.3.3.3 Minimum requirement (network signalled value “NS\_08”) 396

6.6.3.3.4 Minimum requirement (network signalled value “NS\_09”) 396

6.6.3.3.5 Minimum requirement (network signalled value "NS\_12") 397

6.6.3.3.6 Minimum requirement (network signalled value “NS\_13”) 397

6.6.3.3.7 Minimum requirement (network signalled value “NS\_14”) 397

6.6.3.3.8 Minimum requirement (network signalled value “NS\_15”) 398

6.6.3.3.9 Minimum requirement (network signalled value “NS\_16”) 398

6.6.3.3.10 Minimum requirement (network signalled value “NS\_17”) 398

6.6.3.3.11 Minimum requirement (network signalled value “NS\_18”) 398

6.6.3.3.12 Minimum requirement (network signalled value “NS\_19”) 399

6.6.3.3.13 Minimum requirement (network signalled value “NS\_11”) 399

6.6.3.3.14 Minimum requirement (network signalled value “NS\_20”) 399

6.6.3.3.15 Minimum requirement (network signalled value “NS\_21”) 399

6.6.3.3.16 Minimum requirement (network signalled value "NS\_22") 400

6.6.3.3.17 Minimum requirement (network signalled value “NS\_23”) 400

6.6.3.3.18 Void 401

6.6.3.3.19 Minimum requirement (network signalled value "NS\_04") 401

6.6.3.3.20 Minimum requirement (network signalled value “NS\_24”) 401

6.6.3.3.21 Minimum requirement (network signalled value “NS\_25”) 402

6.6.3.3.22 Minimum requirement (network signalled value “NS\_26”) 402

6.6.3.3.23 Minimum requirement (network signalled value “NS\_27” and “NS\_43”) 402

6.6.3.3.24 Minimum requirement (network signalled value “NS\_28”) 402

6.6.3.3.25 Minimum requirement (network signalled value “NS\_29”) 403

6.6.3.3.26 Minimum requirement (network signalled value “NS\_30”) 403

6.6.3.3.27 Minimum requirement (network signalled value “NS\_31”) 404

6.6.3.3.28 Minimum requirement (network signalled value “NS\_36”) 405

6.6.3.3.29 Minimum requirement (network signalled value “NS\_38”) 405

6.6.3.3.30 Minimum requirement (network signalled value “NS\_39”) 405

6.6.3.3.31 Minimum requirement (network signalled value “NS\_40” and “NS\_41”) 406

6.6.3.3.32 Minimum requirement (network signalled value “NS\_42”) 406

6.6.3.3.33 Minimum requirement (network signalled value “NS\_44”) 406

6.6.3.3.34 Minimum requirement (network signalled value “NS\_45”) 406

6.6.3.3.35 Minimum requirement (network signalled value “NS\_56”) 407

6.6.3.3A Additional spurious emissions for CA 407

6.6.3.3A.1 Minimum requirement for CA\_1C (network signalled value "CA\_NS\_01") 408

6.6.3.3A.2 Minimum requirement for CA\_1C (network signalled value "CA\_NS\_02") 408

6.6.3.3A.3 Minimum requirement for CA\_1C (network signalled value "CA\_NS\_03") 408

6.6.3.3A.4 Minimum requirement for CA\_38C (network signalled value "CA\_NS\_05") 409

6.6.3.3A.5 Minimum requirement for CA\_7C (network signalled value "CA\_NS\_06") 409

6.6.3.3A.6 Minimum requirement for CA\_39C and CA\_39C-41A (network signalled value "CA\_NS\_07") 409

6.6.3.3A.7 Minimum requirement for CA\_42C (network signalled value "CA\_NS\_08") 409

6.6.3.3A.8 Minimum requirement for CA\_41C and CA\_41D (network signalled value "CA\_NS\_04") 410

6.6.3.3A.9 Void 410

6.6.3.3A.10 Minimum requirement for CA\_48B and CA\_48C (network signalled value "CA\_NS\_10") 410

6.6.3A Void 410

6.6.3B Spurious emission for UL-MIMO 411

6.6.3C Void 411

6.6.3D Spurious emission for ProSe 411

6.6.3F Spurious emission for category NB1 and NB2 411

6.6.3G Spurious emission for V2X Communication 411

6.6A Void 415

6.6B Void 415

6.7 Transmit intermodulation 415

6.7.1 Minimum requirement 415

6.7.1A Minimum requirement for CA 416

6.7.1B Minimum requirement for UL-MIMO 416

6.7.1F Minimum requirement for category NB1 and NB2 416

6.7.1G Minimum requirement for V2X Communication 417

6.8 Void 417

6.8A Void 417

6.8B Time alignment error for UL-MIMO 417

6.8B.1 Minimum Requirements 417

6.8C Void 418

6.8D Void 418

6.8E Void 418

6.8F Void 418

6.8G Time alignment error 418

7 Receiver characteristics 418

7.1 General 418

7.2 Diversity characteristics 419

7.3 Reference sensitivity power level 419

7.3.1 Minimum requirements (QPSK) 419

7.3.1A Minimum requirements (QPSK) for CA 454

7.3.1B Minimum requirements (QPSK) for UL-MIMO 554

7.3.1D Minimum requirements (QPSK) for ProSe 554

7.3.1E Minimum requirements (QPSK) for UE category 0, M1, M2 and 1bis 556

7.3.1F Minimum requirements for UE category NB1 and NB2 565

7.3.1F.1 Reference sensitivity for UE category NB1 and NB2 565

7.3.1F.2 Void 566

7.3.1G Minimum requirements (QPSK) for V2X 566

7.3.2 Void 568

7.4 Maximum input level 568

7.4.1 Minimum requirements 569

7.4.1A Minimum requirements for CA 569

7.4.1B Minimum requirements for UL-MIMO 570

7.4.1D Minimum requirements for ProSe 570

7.4.1F Minimum requirements for category NB1 and NB2 571

7.4.1G Minimum requirements for V2X 571

7.4A Void 572

7.4A.1 Void 572

7.5 Adjacent Channel Selectivity (ACS) 572

7.5.1 Minimum requirements 572

7.5.1A Minimum requirements for CA 573

7.5.1B Minimum requirements for UL-MIMO 577

7.5.1D Minimum requirements for ProSe 577

7.5.1F Minimum requirements for category NB1 and NB2 578

7.5.1G Minimum requirements for V2X 579

7.6 Blocking characteristics 581

7.6.1 In-band blocking 581

7.6.1.1 Minimum requirements 581

7.6.1.1A Minimum requirements for CA 583

7.6.1.1D Minimum requirements for ProSe 586

7.6.1.1F Minimum requirements for category NB1 and NB2 587

7.6.1.1G Minimum requirements for V2X 587

7.6.2 Out-of-band blocking 589

7.6.2.1 Minimum requirements 589

7.6.2.1A Minimum requirements for CA 591

7.6.2.1D Minimum requirements for ProSe 594

7.6.2.1F Minimum requirements for category NB1 and NB2 594

7.6.2.1G Minimum requirements for V2X 595

7.6.3 Narrow band blocking 596

7.6.3.1 Minimum requirements 596

7.6.3.1A Minimum requirements for CA 597

7.6.3.1D Minimum requirements for ProSe 598

7.6A Void 599

7.6B Blocking characteristics for UL-MIMO 599

7.7 Spurious response 599

7.7.1 Minimum requirements 599

7.7.1A Minimum requirements for CA 600

7.7.1B Minimum requirements for UL-MIMO 601

7.7.1D Minimum requirements for ProSe 601

7.7.1F Minimum requirements for UE category NB1 and NB2 602

7.7.1G Minimum requirements for V2X 602

7.8 Intermodulation characteristics 603

7.8.1 Wide band intermodulation 603

7.8.1.1 Minimum requirements 603

7.8.1A Minimum requirements for CA 604

7.8.1B Minimum requirements for UL-MIMO 607

7.8.1D Minimum requirements for ProSe 607

7.8.1F Minimum requirements for category NB1 and NB2 608

7.8.1G Minimum requirements 608

7.8.2 Void 609

7.9 Spurious emissions 609

7.9.1 Minimum requirements 610

7.9.1A Minimum requirements 610

7.10 Receiver image 611

7.10.1 Void 611

7.10.1A Minimum requirements for CA 611

7.10.1G Minimum requirements for V2X Communication 611

8 Performance requirement 612

8.1 General 612

8.1.1 Receiver antenna capability 612

8.1.1.1 Simultaneous unicast and MBMS operations 613

8.1.1.2 Dual-antenna receiver capability in idle mode 613

8.1.2 Applicability of requirements 613

8.1.2.1 Applicability of requirements for different channel bandwidths 613

8.1.2.2 Definition of CA capability 613

8.1.2.2A Definition of dual connectivity capability 618

8.1.2.3 Applicability and test rules for different CA configurations and bandwidth combination sets 619

8.1.2.3A Applicability and test rules for different dual connectivity configuration and bandwidth combination set 621

8.1.2.3B Applicability and test rules for different TDD-FDD CA configurations and bandwidth combination sets 622

8.1.2.3C Applicability and test rules for SDR tests for 4Rx capable UEs 624

8.1.2.3D Applicability and test rules for different CA with LAA SCell(s) configurations and bandwidth combination sets 624

8.1.2.3E Applicability and test rules for SDR tests for 8Rx capable UEs 625

8.1.2.4 Test coverage for different number of component carriers 626

8.1.2.5 Applicability of performance requirements for Type B receiver 627

8.1.2.6 Applicability of performance requirements for 4Rx capable UEs 627

8.1.2.6.1 Applicability rule and antenna connection for single carrier tests with 2Rx 627

8.1.2.6.2 Applicability rule and antenna connection for CA and DC tests with 2Rx 629

8.1.2.6.3 Applicability rule and antenna connection for single carrier tests with 4Rx 629

8.1.2.6.4 Applicability rule for 256QAM tests 630

8.1.2.6.5 Applicability rule and antenna connection for CA and DC tests with 4Rx 630

8.1.2.6.6 Applicability rule for Type C with 4Rx 634

8.1.2.6.7 Applicability rule for 1024QAM tests 634

8.1.2.7 Applicability of Enhanced Downlink Control Channel Performance Requirements 634

8.1.2.8 Applicability of performance requirements for CDM-multiplexed DM RS with interfering simultaneous transmission (FRC) with multiple CSI-RS configurations 636

8.1.2.8A Applicability of performance requirements for UE supporting coverage enhancement 636

8.1.2.9 Applicability of SDR requirements for CA and LAA 637

8.1.2.10 Applicability of performance requirements for Multi-user Superposed Transmission 638

8.1.2.11 Applicability CRS interference mitigation receivers performance requirements 638

8.1.2.12 Applicability of performance requirements for 8Rx capable UEs 639

8.1.2.12.1 Applicability rule and antenna connection for single carrier PDSCH tests 639

8.1.2.12.2 Applicability rule and antenna connection for control channel tests 645

8.1.2.12.3 Applicability rule and antenna connection for CA and DC tests 645

8.1.3 UE category and UE DL category 646

8.2 Demodulation of PDSCH (Cell-Specific Reference Symbols) 646

8.2.1 FDD (Fixed Reference Channel) 646

8.2.1.1 Single-antenna port performance 647

8.2.1.1.1 Minimum Requirement 647

8.2.1.1.2 Void 653

8.2.1.1.3 Void 653

8.2.1.1.4 Minimum Requirement 1 PRB allocation in presence of MBSFN 653

8.2.1.1.4A Minimum Requirement 1 PRB allocation in presence of FeMBMS Unicast-mixed Cell under CA 653

8.2.1.2 Transmit diversity performance 654

8.2.1.2.1 Minimum Requirement 2 Tx Antenna Port 654

8.2.1.2.2 Minimum Requirement 4 Tx Antenna Port 655

8.2.1.2.3 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS) 655

8.2.1.2.3A Minimum Requirement 2 Tx Antenna Ports (demodulation subframe overlaps with aggressor cell ABS and CRS assistance information are configured) 657

8.2.1.2.4 Enhanced Performance Requirement Type A - 2 Tx Antenna Ports with TM3 interference model 659

8.2.1.2.5 Enhanced Performance Requirement Type B - 2 Tx Antenna Ports with TM2 interference model 661

8.2.1.2.6 Enhanced Performance Requirement Type B - 2 Tx Antenna Ports with TM9 interference model 662

8.2.1.2.7 Minimum Requirement 2 Tx Antenna Port (Superposed transmission) 663

8.2.1.3 Open-loop spatial multiplexing performance 663

8.2.1.3.1 Minimum Requirement 2 Tx Antenna Port 663

8.2.1.3.1A Soft buffer management test 667

8.2.1.3.1B Enhanced Performance Requirement Type C –2Tx Antenna Ports 668

8.2.1.3.1C Enhanced Performance Requirement Type C - 2 Tx Antenna Ports with TM1 interference 669

8.2.1.3.2 Minimum Requirement 4 Tx Antenna Port 670

8.2.1.3.3 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS) 670

8.2.1.3.4 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS and CRS assistance information are configured) 674

8.2.1.3.5 Minimum Requirement 2 Tx Antenna Port (Superposed transmission) 676

8.2.1.3.6 Minimum Requirement 2 Tx Antenna Port (network-based CRS interference mitigation) 677

8.2.1.4 Closed-loop spatial multiplexing performance 678

8.2.1.4.1 Minimum Requirement Single-Layer Spatial Multiplexing 2 Tx Antenna Port 678

8.2.1.4.1A Minimum Requirement Single-Layer Spatial Multiplexing 4 Tx Antenna Port 679

8.2.1.4.1B Enhanced Performance Requirement Type A - Single-Layer Spatial Multiplexing 2 Tx Antenna Port with TM4 interference model 679

8.2.1.4.1C Minimum Requirement Single-Layer Spatial Multiplexing 2 Tx Antenna Ports (demodulation subframe overlaps with aggressor cell ABS and CRS assistance information are configured) 681

8.2.1.4.1D Enhanced Performance Requirement Type B - Single-layer Spatial Multiplexing 2 Tx Antenna Port with TM4 interference model 684

8.2.1.4.1E Minimum Requirement Single-Layer Spatial Multiplexing 2 Tx Antenna Ports with CRS assistance information 686

8.2.1.4.1F Minimum Requirement Single-Layer Spatial Multiplexing 4 Tx Antenna Ports with CRS assistance information 687

8.2.1.4.2 Minimum Requirement Multi-Layer Spatial Multiplexing 2 Tx Antenna Port 688

8.2.1.4.2A Enhanced Performance Requirement Type C – Multi-layer Spatial Multiplexing 2Tx Antenna Ports 689

8.2.1.4.3 Minimum Requirement Multi-Layer Spatial Multiplexing 4 Tx Antenna Port 689

8.2.1.4.3A Minimum Requirement Multi-Layer Spatial Multiplexing 4 Tx Antenna Port for dual connectivity 693

8.2.1.4.4 Minimum Requirement Multi-Layer Spatial Multiplexing 2 Tx Antenna Port (Superposed transmission) 695

8.2.1.5 MU-MIMO 696

8.2.1.6 [Control channel performance: D-BCH and PCH] 696

8.2.1.7 Carrier aggregation with power imbalance 696

8.2.1.7.1 Minimum Requirement 696

8.2.1.8 Intra-band non-contiguous carrier aggregation with timing offset 697

8.2.1.8.1 Minimum Requirement 697

8.2.1.9 HST-SFN performance 698

8.2.1.9.1 Minimum Requirement 698

8.2.1.9.2 Minimum Requirement for Rel-16 further enhanced HST 701

8.2.1.10 Intra-band contiguous carrier aggregation with minimum channel spacing 701

8.2.1.10.1 Minimum Requirement 702

8.2.2 TDD (Fixed Reference Channel) 702

8.2.2.1 Single-antenna port performance 703

8.2.2.1.1 Minimum Requirement 703

8.2.2.1.2 Void 708

8.2.2.1.3 Void 708

8.2.2.1.4 Minimum Requirement 1 PRB allocation in presence of MBSFN 708

8.2.2.2 Transmit diversity performance 708

8.2.2.2.1 Minimum Requirement 2 Tx Antenna Port 708

8.2.2.2.2 Minimum Requirement 4 Tx Antenna Port 709

8.2.2.2.3 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS) 710

8.2.2.2.3A Minimum Requirement 2 Tx Antenna Ports (demodulation subframe overlaps with aggressor cell ABS and CRS assistance information are configured) 711

8.2.2.2.4 Enhanced Performance Requirement Type A – 2 Tx Antenna Ports with TM3 interference model 713

8.2.2.2.5 Minimum Requirement 2 Tx Antenna Port (when *EIMTA-MainConfigServCell-r12* is configured) 715

8.2.2.2.6 Enhanced Performance Requirement Type B - 2 Tx Antenna Ports with TM2 interference model 715

8.2.2.2.7 Enhanced Performance Requirement Type B - 2 Tx Antenna Ports with TM9 interference model 717

8.2.2.2.8 Minimum Requirement 2 Tx Antenna Port (Superposed transmission) 718

8.2.2.3 Open-loop spatial multiplexing performance 719

8.2.2.3.1 Minimum Requirement 2 Tx Antenna Port 719

8.2.2.3.1A Soft buffer management test 722

8.2.2.3.1B Enhanced Performance Requirement Type C - 2Tx Antenna Ports 722

8.2.2.3.1C Enhanced Performance Requirement Type C - 2 Tx Antenna Ports with TM1 interference 723

8.2.2.3.2 Minimum Requirement 4 Tx Antenna Port 724

8.2.2.3.3 Minimum Requirement 2Tx antenna port (demodulation subframe overlaps with aggressor cell ABS) 725

8.2.2.3.4 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS and CRS assistance information are configured) 729

8.2.2.3.5 Minimum Requirement 2 Tx Antenna Port (Superposed transmission) 731

8.2.2.3.6 Minimum Requirement 2 Tx Antenna Port (network-based CRS interference mitigation) 732

8.2.2.4 Closed-loop spatial multiplexing performance 733

8.2.2.4.1 Minimum Requirement Single-Layer Spatial Multiplexing 2 Tx Antenna Port 733

8.2.2.4.1A Minimum Requirement Single-Layer Spatial Multiplexing 4 Tx Antenna Port 734

8.2.2.4.1B Enhanced Performance Requirement Type A – Single-Layer Spatial Multiplexing 2 Tx Antenna Port with TM4 interference model 734

8.2.2.4.1C Minimum Requirement Single-Layer Spatial Multiplexing 2 Tx Antenna Ports (demodulation subframe overlaps with aggressor cell ABS and CRS assistance information are configured) 736

8.2.2.4.1D Enhanced Performance Requirement Type B - Single-layer Spatial Multiplexing 2 Tx Antenna Port with TM4 interference model 738

8.2.2.4.1E Minimum Requirement Single-Layer Spatial Multiplexing 2 Tx Antenna Ports with CRS assistance information 740

8.2.2.4.1F Minimum Requirement Single-Layer Spatial Multiplexing 4 Tx Antenna Ports with CRS assistance information 741

8.2.2.4.2 Minimum Requirement Multi-Layer Spatial Multiplexing 2 Tx Antenna Port 743

8.2.2.4.2A Enhanced Performance Requirement Type C Multi-Layer Spatial Multiplexing 2 Tx Antenna Port 743

8.2.2.4.3 Minimum Requirement Multi-Layer Spatial Multiplexing 4 Tx Antenna Port 744

8.2.2.4.3A Minimum Requirement Multi-Layer Spatial Multiplexing 4 Tx Antenna Port for dual connectivity 748

8.2.2.4.4 Void 749

8.2.2.4.5 Minimum Requirement Multi-Layer Spatial Multiplexing 2 Tx Antenna Port (Superposed transmission) 749

8.2.2.5 MU-MIMO 750

8.2.2.6 [Control channel performance: D-BCH and PCH] 750

8.2.2.7 Carrier aggregation with power imbalance 750

8.2.2.7.1 Minimum Requirement 750

8.2.2.8 Intra-band contiguous carrier aggregation with minimum channel spacing 751

8.2.2.8.1 Minimum Requirement 751

8.2.2.9 HST-SFN performance 752

8.2.2.9.1 Minimum Requirement 752

8.2.2.9.2 Minimum Requirement for Rel-16 further enhanced HST 754

8.2.3 TDD FDD CA (Fixed Reference Channel) 755

8.2.3.1 Single-antenna port performance 756

8.2.3.1.1 Minimum Requirement for FDD PCell 756

8.2.3.1.2 Minimum Requirement for TDD PCell 760

8.2.3.2 Open-loop spatial multiplexing performance 2Tx Antenna port 764

8.2.3.2.1 Minimum Requirement for FDD PCell 764

8.2.3.2.1A Soft buffer management test for FDD PCell 768

8.2.3.2.2 Minimum Requirement for TDD PCell 769

8.2.3.2.2A Soft buffer management test for TDD PCell 773

8.2.3.3 Closed-loop spatial multiplexing performance 4Tx Antenna Port 774

8.2.3.3.1 Minimum Requirement for FDD PCell 774

8.2.3.3.2 Minimum Requirement for TDD PCell 778

8.2.3.4 Minimum Requirement for Closed-loop spatial multiplexing performance 4Tx Antenna Port for dual connectivity 782

8.2.3.5 HST-SFN performance 784

8.2.3.5.0 General 784

8.2.3.5.1 Minimum Requirement for FDD PCell 784

8.2.3.5.2 Minimum Requirement for TDD PCell 787

8.2.4 LAA 790

8.2.4.1 Closed-loop spatial multiplexing performance 4Tx Antenna Port 790

8.2.4.1.1 FDD PCell (FDD single carrier) 790

8.2.4.1.2 TDD PCell (TDD single carrier) 794

8.3 Demodulation of PDSCH (User-Specific Reference Symbols) 797

8.3.1 FDD 797

8.3.1.1 Single-layer Spatial Multiplexing 798

8.3.1.1A Enhanced Performance Requirement Type A – Single-layer Spatial Multiplexing with TM9 interference model 800

8.3.1.1B Single-layer Spatial Multiplexing (demodulation subframe overlaps with aggressor cell ABS and CRS assistance information are configured) 803

8.3.1.1C Enhanced Performance Requirement Type B – Single-layer Spatial Multiplexing with TM9 interference model 806

8.3.1.1D Enhanced Performance Requirement Type B – Single-layer Spatial Multiplexing with CRS interference model 808

8.3.1.1E Enhanced Performance Requirement Type B – Single-layer Spatial Multiplexing with TM3 interference model 809

8.3.1.1F Enhanced Performance Requirement Type B – Single-layer Spatial Multiplexing with TM10 serving cell configuration and TM9 interference model 810

8.3.1.1G Single-layer Spatial Multiplexing (CRS assistance information is configured) 812

8.3.1.1H Single-layer Spatial Multiplexing (With Enhanced DMRS table configured) 814

8.3.1.1I Single-layer Spatial Multiplexing (with assistance information for simultaneous transmition interfering PDSCH) 815

8.3.1.2 Dual-Layer Spatial Multiplexing 817

8.3.1.2A Enhanced Performance Requirement Type C - Dual-Layer Spatial Multiplexing 818

8.3.1.3 Performance requirements for DCI format 2D and non Quasi Co-located Antenna Ports 819

8.3.1.3.1 Minimum requirement with Same Cell ID (with single NZP CSI-RS resource) 819

8.3.1.3.2 Minimum requirements with Same Cell ID (with multiple NZP CSI-RS resources) 821

8.3.1.3.3 Minimum requirement with Different Cell ID and Colliding CRS (with single NZP CSI-RS resource) 823

8.3.1.3.4 Minimum requirement with Different Cell ID and non-colliding CRS (with single NZP CSI-RS resource and CRS assistance information is configured) 825

8.3.1.3.5 Minimum requirements with different Cell ID and non-colliding CRS (with multiple NZP CSI-RS resources and CRS assistance information is configured) 827

8.3.1.3.6 Minimum requirements for QCL Type C and 2 Layers Spatial Multiplexing 830

8.3.1.4 Performance Requirements for semiOpenLoop transmission 832

8.3.2 TDD 834

8.3.2.1 Single-layer Spatial Multiplexing 834

8.3.2.1A Single-layer Spatial Multiplexing (with multiple CSI-RS configurations) 836

8.3.2.1B Enhanced Performance Requirement Type A – Single-layer Spatial Multiplexing with TM9 interference model 838

8.3.2.1C Single-layer Spatial Multiplexing (demodulation subframe overlaps with aggressor cell ABS and CRS assistance information are configured) 841

8.3.2.1D Enhanced Performance Requirement Type B – Single-layer Spatial Multiplexing with TM9 interference 844

8.3.2.1E Enhanced Performance Requirement Type B – Single-layer Spatial Multiplexing with CRS interference model 846

8.3.2.1F Enhanced Performance Requirement Type B – Single-layer Spatial Multiplexing with TM3 interference 848

8.3.2.1G Enhanced Performance Requirement Type B – Single-layer Spatial Multiplexing with TM10 serving cell configuration and TM9 interference model 849

8.3.2.1H Single-layer Spatial Multiplexing (CRS assistance information is configured) 851

8.3.2.1I Single-layer Spatial Multiplexing (With Enhanced DMRS table configured) 853

8.3.2.1J Single-layer Spatial Multiplexing (with assistance information for simultaneous transmition interfering PDSCH) 854

8.3.2.2 Dual-Layer Spatial Multiplexing 856

8.3.2.2A Enhanced Performance Requirement Type C - Dual-Layer Spatial Multiplexing 856

8.3.2.3 Dual-Layer Spatial Multiplexing (with multiple CSI-RS configurations) 857

8.3.2.4 Performance requirements for DCI format 2D and non Quasi Co-located Antenna Ports 858

8.3.2.4.1 Minimum requirement with Same Cell ID (with single NZP CSI-RS resource) 858

8.3.2.4.2 Minimum requirements with Same Cell ID (with multiple NZP CSI-RS resources) 860

8.3.2.4.3 Minimum requirement with Different Cell ID and Colliding CRS (with single NZP CSI-RS resource) 862

8.3.2.4.4 Minimum requirement with Different Cell ID and non-Colliding CRS (with single NZP CSI-RS resource and CRS assistance information is configured) 864

8.3.2.4.5 Minimum requirements with different Cell ID and non-colliding CRS (with multiple NZP CSI-RS resources and CRS assistance information is configured) 866

8.3.2.4.6 Minimum requirements for QCL Type C and 2 Layers Spatial Multiplexing 869

8.3.2.5 Performance Requirements for semiOpenLoop transmission 871

8.3.3 LAA 873

8.3.3.1 Dual-Layer Spatial Multiplexing with DM-RS 873

8.3.3.1.1 FDD PCell (FDD single carrier) 873

8.3.3.1.2 TDD Pcell (TDD single carrier) 878

8.4 Demodulation of PDCCH/PCFICH 882

8.4.1 FDD 882

8.4.1.1 Single-antenna port performance 883

8.4.1.2 Transmit diversity performance 883

8.4.1.2.1 Minimum Requirement 2 Tx Antenna Port 883

8.4.1.2.2 Minimum Requirement 4 Tx Antenna Port 883

8.4.1.2.3 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS) 884

8.4.1.2.4 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS and CRS assistance information are configured) 889

8.4.1.2.5 Enhanced Downlink Control Channel Performance Requirement Type A - 2 Tx Antenna Port under Asynchronous Network 895

8.4.1.2.6 Enhanced Downlink Control Channel Performance Requirement Type A - 2 Tx Antenna Port with Non-Colliding CRS Dominant Interferer 896

8.4.1.2.7 Enhanced Downlink Control Channel Performance Requirement Type B - 2 Tx Antenna Port with Colliding CRS Dominant Interferer 897

8.4.1.2.8 Enhanced Downlink Control Channel Performance Requirement Type B - 2 Tx Antenna Port with Non-Colliding CRS Dominant Interferer 898

8.4.1.2.9 Enhanced Downlink Control Channel Performance Requirement Type A - 4 Tx Antenna Port with Non-Colliding CRS Dominant Interferer 899

8.4.2 TDD 900

8.4.2.1 Single-antenna port performance 901

8.4.2.2 Transmit diversity performance 901

8.4.2.2.1 Minimum Requirement 2 Tx Antenna Port 901

8.4.2.2.2 Minimum Requirement 4 Tx Antenna Port 902

8.4.2.2.3 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS) 902

8.4.2.2.4 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS and CRS assistance information are configured) 906

8.4.2.2.5 Enhanced Downlink Control Channel Performance Requirement Type A - 2 Tx Antenna Port with Colliding CRS Dominant Interferer 910

8.4.2.2.6 Enhanced Downlink Control Channel Performance Requirement Type A - 2 Tx Antenna Port with Non-Colliding CRS Dominant Interferer 911

8.4.2.2.7 Enhanced Downlink Control Channel Performance Requirement Type B - 2 Tx Antenna Port with Colliding CRS Dominant Interferer 912

8.4.2.2.8 Enhanced Downlink Control Channel Performance Requirement Type B - 2 Tx Antenna Port with Non-Colliding CRS Dominant Interferer 913

8.4.2.2.9 Enhanced Downlink Control Channel Performance Requirement Type A - 4 Tx Antenna Port with Non-Colliding CRS Dominant Interferer 914

8.4.3 LAA 915

8.4.3.1 Transmit diversity performance 915

8.4.3.1.1 FDD Pcell (FDD single carrier) 915

8.4.3.1.2 TDD Pcell (TDD single carrier) 916

8.5 Demodulation of PHICH 917

8.5.1 FDD 918

8.5.1.1 Single-antenna port performance 918

8.5.1.2 Transmit diversity performance 918

8.5.1.2.1 Minimum Requirement 2 Tx Antenna Port 918

8.5.1.2.2 Minimum Requirement 4 Tx Antenna Port 919

8.5.1.2.3 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS) 919

8.5.1.2.4 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS and CRS assistance information are configured) 921

8.5.1.2.5 Enhanced Downlink Control Channel Performance Requirement Type A - 2 Tx Antenna Ports under Asynchronous Network 924

8.5.1.2.6 Enhanced Downlink Control Channel Performance Requirement Type A - 2 Tx Antenna Ports with Non-Colliding CRS Dominant Interferer 925

8.5.1.2.7 Enhanced Downlink Control Channel Performance Requirement Type B - 2 Tx Antenna Ports with Colliding CRS Dominant Interferer 926

8.5.1.2.8 Enhanced Downlink Control Channel Performance Requirement Type B - 2 Tx Antenna Ports with Non-Colliding CRS Dominant Interferer 927

8.5.2 TDD 928

8.5.2.1 Single-antenna port performance 929

8.5.2.2 Transmit diversity performance 929

8.5.2.2.1 Minimum Requirement 2 Tx Antenna Port 929

8.5.2.2.2 Minimum Requirement 4 Tx Antenna Port 930

8.5.2.2.3 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS) 930

8.5.2.2.4 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS and CRS assistance information are configured) 932

8.5.2.2.5 Enhanced Downlink Control Channel Performance Requirement Type A - 2 Tx Antenna Ports with Colliding CRS Dominant Interferer 934

8.5.2.2.6 Enhanced Downlink Control Channel Performance Requirement Type A - 2 Tx Antenna Ports with Non-Colliding CRS Dominant Interferer 935

8.5.2.2.7 Enhanced Downlink Control Channel Performance Requirement Type B - 2 Tx Antenna Ports with Colliding CRS Dominant Interferer 936

8.5.2.2.8 Enhanced Downlink Control Channel Performance Requirement Type B - 2 Tx Antenna Ports with Non-Colliding CRS Dominant Interferer 937

8.6 Demodulation of PBCH 938

8.6.1 FDD 938

8.6.1.1 Single-antenna port performance 938

8.6.1.2 Transmit diversity performance 939

8.6.1.2.1 Minimum Requirement 2 Tx Antenna Port 939

8.6.1.2.2 Minimum Requirement 4 Tx Antenna Port 939

8.6.1.2.3 Minimum Requirement 2 Tx Antenna Port under Time Domain Measurement Resource Restriction with CRS Assistance Information 939

8.6.2 TDD 941

8.6.2.1 Single-antenna port performance 941

8.6.2.2 Transmit diversity performance 941

8.6.2.2.1 Minimum Requirement 2 Tx Antenna Port 941

8.6.2.2.2 Minimum Requirement 4 Tx Antenna Port 941

8.6.2.2.3 Minimum Requirement 2 Tx Antenna Port under Time Domain Measurement Resource Restriction with CRS Assistance Information 942

8.7 Sustained downlink data rate provided by lower layers 943

8.7.1 FDD (single carrier and CA) 943

8.7.2 TDD (single carrier and CA) 960

8.7.3 FDD (EPDCCH scheduling) 964

8.7.4 TDD (EPDCCH scheduling) 966

8.7.5 TDD FDD CA 968

8.7.5.1 Minimum Requirement FDD PCell 969

8.7.5.2 Minimum Requirement TDD PCell 977

8.7.6 FDD (DC) 986

8.7.7 TDD (DC) 993

8.7.8 TDD FDD (DC) 996

8.7.9 FDD (4 Rx) 999

8.7.10 TDD (4 Rx) 1001

8.7.11 TDD FDD CA (4 Rx) 1003

8.7.11.1 Void 1005

8.7.12 LAA 1005

8.7.12.1 FDD CA in licensed bands 1005

8.7.12.2 TDD CA in licensed bands 1007

8.7.12.3 TDD-FDD CA in licensed bands 1009

8.7.13 FDD DC (4 Rx) 1012

8.7.14 TDD DC (4 Rx) 1013

8.7.15 TDD FDD DC (4 Rx) 1015

8.7.16 FDD (1024QAM and up to 4Rx supported) 1017

8.7.17 TDD (1024QAM and up to 4 Rx supported) 1020

8.7.18 TDD FDD CA (1024QAM and up to 4 Rx supported) 1022

8.7.19 TDD (8 Rx) 1024

8.8 Demodulation of EPDCCH 1026

8.8.1 Distributed Transmission 1026

8.8.1.1 FDD 1026

8.8.1.1.1 Void 1027

8.8.1.2 TDD 1027

8.8.1.2.1 Void 1028

8.8.2 Localized Transmission with TM9 1028

8.8.2.1 FDD 1028

8.8.2.1.1 Void 1029

8.8.2.1.2 Void 1030

8.8.2.2 TDD 1030

8.8.2.2.1 Void 1031

8.8.2.2.2 Void 1031

8.8.3 Localized transmission with TM10 Type B quasi co-location type 1031

8.8.3.1 FDD 1031

8.8.3.2 TDD 1034

8.8.4 Enhanced Downlink Control Channel Performance Requirements Type A - Localized Transmission with CRS Interference Model 1037

8.8.4.1 FDD 1037

8.8.4.2 TDD 1038

8.8.5 Enhanced Downlink Control Channel Performance Requirements Type A - Distributed Transmission with TM9 Interference Model 1040

8.8.5.1 TDD 1040

8.8.6 Enhanced Downlink Control Channel Performance Requirements Type A - Distributed Transmission with TM3 Interference Model 1041

8.8.6.1 FDD 1041

8.9 Demodulation (single receiver antenna) 1042

8.9.1 PDSCH 1042

8.9.1.1 FDD and half-duplex FDD (Fixed Reference Channel) 1042

8.9.1.1.1 Transmit diversity performance (Cell-Specific Reference Symbols) 1042

8.9.1.1.2 Closed-loop spatial multiplexing performance (Cell-Specific Reference Symbols) 1043

8.9.1.1.3 Closed-loop spatial multiplexing performance (User-Specific Reference Symbols) 1045

8.9.1.2 TDD (Fixed Reference Channel) 1048

8.9.1.2.1 Transmit diversity performance (Cell-Specific Reference Symbols) 1048

8.9.1.2.2 Closed-loop spatial multiplexing performance (Cell-Specific Reference Symbols) 1049

8.9.1.2.3 Closed-loop spatial multiplexing performance (User-Specific Reference Symbols) 1052

8.9.2 PHICH 1054

8.9.2.1 FDD and half-duplex FDD 1054

8.9.2.1.1 Transmit diversity performance 1054

8.9.2.2 TDD 1054

8.9.2.2.1 Transmit diversity performance 1054

8.9.3 PBCH 1055

8.9.3.1 FDD and half-duplex FDD 1055

8.9.3.1.1 Transmit diversity performance 1055

8.9.3.2 TDD 1055

8.9.3.2.1 Transmit diversity performance 1055

8.9.4 PDCCH/PCFICH 1055

8.9.4.1 FDD and half-duplex FDD 1055

8.9.4.1.1 Enhanced Downlink Control Channel Performance Requirement Type A - 2 Tx Antenna Port with Non-Colliding CRS Dominant Interferer 1055

8.9.4.1.2 Enhanced Downlink Control Channel Performance Requirement Type A - 4 Tx Antenna Port with Non-Colliding CRS Dominant Interferer 1056

8.9.4.2 TDD 1057

8.9.4.2.1 Enhanced Downlink Control Channel Performance Requirement Type A - 2 Tx Antenna Port with Non-Colliding CRS Dominant Interferer 1057

8.9.4.2.2 Enhanced Downlink Control Channel Performance Requirement Type A - 4 Tx Antenna Port with Non-Colliding CRS Dominant Interferer 1058

8.10 Demodulation (4 receiver antenna ports) 1059

8.10.1 PDSCH 1059

8.10.1.1 FDD (Fixed Reference Channel) 1059

8.10.1.1.1 Transmit diversity performance with 2Tx Antenna Ports (Cell-Specific Reference Symbols) 1060

8.10.1.1.1A Transmit diversity performance wit Enhanced Performance Requirement Type A - 2 Tx Antenna Ports with TM3 interference model 1061

8.10.1.1.2 Open-loop spatial multiplexing performance with 2Tx Antenna Ports (Cell-Specific Reference Symbols) 1062

8.10.1.1.3 Closed-loop spatial multiplexing Enhanced Performance Requirements Type A - Single-Layer Spatial Multiplexing 2 Tx Antenna Port with TM4 interference model (Cell-Specific Reference Symbols) 1062

8.10.1.1.4 Closed-loop spatial multiplexing performance, Dual-Layer Spatial Multiplexing 4 Tx Antenna Port (Cell-Specific Reference Symbols) 1063

8.10.1.1.4A Enhanced Performance Requirement Type C - Dual-Layer Spatial Multiplexing with 2Tx Antenna Ports 1064

8.10.1.1.5 Enhanced Performance Requirement Type A – Single-layer Spatial Multiplexing with TM9 interference model (User-Specific Reference Symbols) 1065

8.10.1.1.5A Single-layer Spatial Multiplexing (User-Specific Reference Symbols) 1068

8.10.1.1.5B Single-layer Spatial Multiplexing (With Enhanced DMRS table configured) 1069

8.10.1.1.6 Dual-Layer Spatial Multiplexing (User-Specific Reference Symbols) 1070

8.10.1.1.6A Enhanced Performance Requirement Type C - Dual-Layer Spatial Multiplexing 1072

8.10.1.1.6B Dual-Layer Spatial Multiplexing with altCQI-Table-1024QAM configured (User-Specific Reference Symbols) 1073

8.10.1.1.7 Open-loop spatial multiplexing, 3 Layer Multiplexing with 4 Tx Antenna Ports (Cell-Specific Reference Symbols) 1074

8.10.1.1.7A Enhanced Performance Requirement Type C - Open-loop spatial multiplexing, 3 Layer Multiplexing with 4 Tx Antenna Ports (Cell-Specific Reference Symbols) 1074

8.10.1.1.8 Closed-loop spatial multiplexing performance, 4 Layers spatial multiplexing 4 Tx antennas (Cell-Specific Reference Symbols) 1075

8.10.1.1.9 4 Layer Spatial Multiplexing (User-Specific Reference Symbols) 1075

8.10.1.1.9A Enhanced Performance Requirement Type C - 4 Layer Spatial Multiplexing (User-Specific Reference Symbols) 1077

8.10.1.1.10 Closed loop spatial multiplexing performance - Single-Layer Spatial Multiplexing 2 Tx Antenna Port with CRS assistance information (Cell-Specific Reference Symbols) 1078

8.10.1.1.11 Closed loop spatial multiplexing performance - Single-Layer Spatial Multiplexing 4 Tx Antenna Port with CRS assistance information (Cell-Specific Reference Symbols) 1079

8.10.1.1.12 Closed loop spatial multiplexing performance - Single-Layer Spatial Multiplexing with CRS assistance information (User-Specific Reference Symbols) 1080

8.10.1.1.13 Performance requirements for DCI format 2D and non Quasi Co-located Antenna Ports 1081

8.10.1.1.14 HST-SFN performance 1085

8.10.1.2 TDD (Fixed Reference Channel) 1085

8.10.1.2.1 Transmit diversity performance with 2Tx Antenna Ports (Cell-Specific Reference Symbols) 1086

8.10.1.2.1A Transmit diversity performance with Enhanced Performance Requirement Type A – 2 Tx Antenna Ports with TM3 interference model 1087

8.10.1.2.2 Open-loop spatial multiplexing performance with 2Tx Antenna Ports (Cell-Specific Reference Symbols) 1088

8.10.1.2.3 Closed-loop spatial multiplexing Enhanced Performance Requirements Type A - Single-Layer Spatial Multiplexing 2 Tx Antenna Port with TM4 interference model (Cell-Specific Reference Symbols) 1088

8.10.1.2.4 Closed-loop spatial multiplexing performance, Dual-Layer Spatial Multiplexing 4 Tx Antenna Ports (Cell-Specific Reference Symbols) 1089

8.10.1.2.4A Enhanced Performance Requirement Type C - Dual-Layer Spatial Multiplexing with 2Tx Antenna Ports 1090

8.10.1.2.5 Enhanced Performance Requirement Type A – Single-layer Spatial Multiplexing with TM9 interference model (User-Specific Reference Symbols) 1091

8.10.1.2.5A Single-layer Spatial Multiplexing (with multiple CSI-RS configurations) 1094

8.10.1.2.5B Single-layer Spatial Multiplexing (With Enhanced DMRS table configured) 1095

8.10.1.2.6 Dual-Layer Spatial Multiplexing (User-Specific Reference Symbols) 1096

8.10.1.2.6A Enhanced Performance Requirement Type C - Dual-Layer Spatial Multiplexing 1098

8.10.1.2.6B Dual-Layer Spatial Multiplexing with altCQI-Table-1024QAM configured (User-Specific Reference Symbols) 1099

8.10.1.2.7 Open-loop spatial multiplexing, 3 Layer Multiplexing with 4 Tx Antenna Ports (Cell-Specific Reference Symbols) 1100

8.10.1.2.7A Enhanced Performance Requirement Type C - Open-loop spatial multiplexing, 3 Layer Multiplexing with 4 Tx Antenna Ports (Cell-Specific Reference Symbols) 1100

8.10.1.2.8 Closed-loop spatial multiplexing performance, 4 Layers spatial multiplexing 4 Tx antennas 1101

8.10.1.2.9 4 Layer Spatial Multiplexing (User-Specific Reference Symbols) 1102

8.10.1.2.9A Enhanced Performance Requirement Type C - 4 Layer Spatial Multiplexing (User-Specific Reference Symbols) 1103

8.10.1.2.10 Closed loop spatial multiplexing performance - Single-Layer Spatial Multiplexing 2 Tx Antenna Port with CRS assistance information (Cell-Specific Reference Symbols) 1104

8.10.1.2.11 Closed loop spatial multiplexing performance - Single-Layer Spatial Multiplexing 4 Tx Antenna Port with CRS assistance information (Cell-Specific Reference Symbols) 1106

8.10.1.2.12 Closed loop spatial multiplexing performance - Single-Layer Spatial Multiplexing with CRS assistance information (User-Specific Reference Symbols) 1107

8.10.1.2.13 Performance requirements for DCI format 2D and non Quasi Co-located Antenna Ports 1109

8.10.1.2.14 HST-SFN performance 1113

8.10.2 PDCCH/PCFICH 1114

8.10.2.1 FDD 1114

8.10.2.1.1 Single-antenna port performance 1114

8.10.2.1.2 Transmit diversity performance with 2 Tx Antenna Ports 1114

8.10.2.1.3 Transmit diversity performance with 4 Tx Antenna Ports 1114

8.10.2.1.4 Enhanced Downlink Control Channel Performance Requirement Type A - 4 Tx Antenna Port with Non-Colliding CRS Dominant Interferer 1115

8.10.2.2 TDD 1116

8.10.2.2.1 Single-antenna port performance 1116

8.10.2.2.2 Transmit diversity performance with 2 Tx Antenna Ports 1117

8.10.2.2.3 Transmit diversity performance with 4 Tx Antenna Ports 1117

8.10.2.2.4 Enhanced Downlink Control Channel Performance Requirement Type A - 4 Tx Antenna Port with Non-Colliding CRS Dominant Interferer 1117

8.10.3 PHICH 1118

8.10.3.1 FDD 1118

8.10.3.1.1 Single Tx Antenna Port performance 1119

8.10.3.1.2 Transmit diversity performance with 2 Tx Antenna Ports 1119

8.10.3.1.3 Transmit diversity performance with 4 Tx Antenna Ports 1119

8.10.3.2 TDD 1120

8.10.3.2.1 Single Tx Antenna Port performance 1120

8.10.3.2.2 Transmit diversity performance with 2 Tx Antenna Ports 1121

8.10.3.2.3 Transmit diversity performance with 4 Tx Antenna Ports 1121

8.10.4 ePDCCH 1121

8.10.4.1 Distributed Transmission with 4Rx 1121

8.10.4.1.1 FDD 1121

8.10.4.1.2 TDD 1122

8.10.4.2 Localized Transmission with TM9 and 4Rx 1123

8.10.4.2.1 FDD 1123

8.10.4.2.2 TDD 1124

8.11 Demodulation (UE supporting coverage enhancement) 1125

8.11.1 PDSCH 1126

8.11.1.1 FDD and half-duplex FDD (Fixed Reference Channel) 1126

8.11.1.1.1 Closed-loop spatial multiplexing performance (Cell-Specific Reference Symbols) 1126

8.11.1.1.2 Closed-loop spatial multiplexing performance (User-Specific Reference Symbols) 1130

8.11.1.1.3 Transmit diversity performance (Cell-Specific Reference Symbols) 1132

8.11.1.2 TDD (Fixed Reference Channel) 1137

8.11.1.2.1 Closed-loop spatial multiplexing performance (Cell-Specific Reference Symbols) 1137

8.11.1.2.2 Closed-loop spatial multiplexing performance (User-Specific Reference Symbols) 1142

8.11.1.2.3 Transmit diversity performance (Cell-Specific Reference Symbols) 1144

8.11.2 MPDCCH 1148

8.11.2.1 FDD and half-duplex FDD 1149

8.11.2.1.1 CE Mode A 1150

8.11.2.1.2 CE Mode B 1151

8.11.2.1.3 CE Mode A with TM9 interference model 1151

8.11.2.1.4 CE Mode A with CRS interference model 1153

8.11.2.1.5 CE Mode A and CE Mode B when CRS-ChEstMPDCCH-Config is configured 1154

8.11.2.2.5 CE Mode A and CE Mode B when CRS-ChEstMPDCCH-Config is configured 1155

8.11.2.2 TDD 1157

8.11.2.2.1 CE Mode A 1158

8.11.2.2.2 CE Mode B 1159

8.11.2.2.3 CE Mode A with TM9 interference model 1159

8.11.2.2.4 CE Mode A with CRS interference model 1160

8.11.3 PBCH 1161

8.11.3.1 FDD and half-duplex FDD 1162

8.11.3.1.1 Transmit diversity performance 1162

8.11.3.2 TDD 1163

8.11.3.2.1 Transmit diversity performance 1163

8.12 Demodulation of Narrowband IoT 1163

8.12.1 NPDSCH 1163

8.12.1.1.1 Minimum Requirements for In-band 1164

8.12.1.1.2 Minimum Requirements for Standalone/Guard-band 1165

8.12.1.1.3 Minimum Requirements for Standalone for UE Category NB2 1166

8.12.1.1.4 Minimum Requirements for Standalone for UE with multiple TBs interleaved transmission 1167

8.12.1.2 TDD 1168

8.12.1.2.1 Minimum Requirements for In-band 1168

8.12.1.2.2 Minimum Requirements for Standalone/Guard-band 1169

8.12.1.2.3 Minimum Requirements for Standalone for UE Category NB2 1170

8.12.2 NPDCCH 1170

8.12.2.1 Half-duplex FDD 1170

8.12.2.1.1 Single-antenna performance 1171

8.12.2.1.2 Transmit diversity performance 1172

8.12.2.2 TDD 1172

8.12.2.2.1 Single-antenna performance 1174

8.12.2.2.2 Transmit diversity performance 1174

8.12.3 Demodulation of NPBCH 1174

8.12.3.1 HD-FDD 1175

8.12.3.1.1 Single-antenna port performance with single NPBCH TTI 1175

8.12.3.1.2 Transmit diversity performance 1175

8.12.3.2 TDD 1175

8.12.3.2.1 Single-antenna port performance with single NPBCH TTI 1176

8.12.3.2.2 Transmit diversity performance 1176

8.13 Demodulation of PDSCH CA and DC(4 receiver antenna ports) 1176

8.13.1 FDD (CA and DC) 1176

8.13.1.1 Closed-loop spatial multiplexing performance 1176

8.13.1.1.1 Minimum Requirement Multi-Layer Spatial Multiplexing 4 Tx Antenna Port 1176

8.13.1.1.2 Minimum Requirement Multi-Layer Spatial Multiplexing 4 Tx Antenna Port for dual connectivity 1180

8.13.1.1.3 Minimum Requirement Multi-Layer Spatial Multiplexing 4 Tx Antenna Port with 256QAM 1182

8.13.1.1.4 Minimum Requirement Four-Layer Spatial Multiplexing 4 Tx Antenna Port 1184

8.13.1.2 Dual-Layer Spatial Multiplexing (User-Specific Reference Symbols) 1185

8.13.1.2.1 Minimum Requirement Dual-Layer Spatial Multiplexing 2 Tx Antenna Port 1185

8.13.1.3 Enhanced Performance Requirements Type A Closed-loop spatial multiplexing 1188

8.13.1.3.1 Minimum Requirement Single-Layer Spatial Multiplexing 2 Tx Antenna Port with TM4 interference model (Cell-Specific Reference Symbols) 1188

8.13.1.4 Enhanced Performance Requirement Type A - Single-layer Spatial Multiplexing (User-Specific Reference Symbols) 1190

8.13.1.4.1 Minimum Requirement Enhanced Performance Requirement Type A – Single-layer Spatial Multiplexing with TM9 interference model (User-Specific Reference Symbols) 1190

8.13.2 TDD (CA and DC) 1193

8.13.2.1 Closed-loop spatial multiplexing performance 1194

8.13.2.1.1 Minimum Requirement Multi-Layer Spatial Multiplexing 4 Tx Antenna Port 1194

8.13.2.1.2 Minimum Requirement Multi-Layer Spatial Multiplexing 4 Tx Antenna Port for dual connectivity 1196

8.13.2.1.3 Minimum Requirement Multi-Layer Spatial Multiplexing 4 Tx Antenna Port with 256QAM 1197

8.13.2.1.4 Minimum Requirement Four-Layer Spatial Multiplexing 4 Tx Antenna Port 1198

8.13.2.2 Dual-Layer Spatial Multiplexing (User-Specific Reference Symbols) 1200

8.13.2.2.1 Minimum Requirement Dual-Layer Spatial Multiplexing 2 Tx Antenna Port 1200

8.13.2.4 Enhanced Performance Requirement Type A - Single-layer Spatial Multiplexing (User-Specific Reference Symbols) 1204

8.13.2.4.1 Minimum Requirement Enhanced Performance Requirement Type A – Single-layer Spatial Multiplexing with TM9 interference model (User-Specific Reference Symbols) 1204

8.13.3 TDD-FDD (CA and DC) 1206

8.13.3.1 Closed-loop spatial multiplexing performance 4Tx Antenna Port 1206

8.13.3.1.1 Minimum Requirement for FDD PCell 1206

8.13.3.1.2 Minimum Requirement for TDD PCell 1210

8.13.3.2 Dual-Layer Spatial Multiplexing (User-Specific Reference Symbols) 1214

8.13.3.2.1 Minimum Requirement Dual-Layer Spatial Multiplexing 2 Tx Antenna Port for FDD PCell 1214

8.13.3.2.2 Minimum Requirement Dual-Layer Spatial Multiplexing 2 Tx Antenna Port for TDD PCell 1217

8.13.3.3 Enhanced Performance Requirements Type A Closed-loop spatial multiplexing 1220

8.13.3.3.1 Minimum Requirement Single-Layer Spatial Multiplexing 2 Tx Antenna Port with TM4 interference model (Cell-Specific Reference Symbols) for FDD PCell 1220

8.13.3.3.2 Minimum Requirement Single-Layer Spatial Multiplexing 2 Tx Antenna Port with TM4 interference model (Cell-Specific Reference Symbols) for TDD PCell 1222

8.13.3.4 Enhanced Performance Requirement Type A - Single-layer Spatial Multiplexing (User-Specific Reference Symbols) 1224

8.13.3.4.1 Minimum Requirement Enhanced Performance Requirement Type A – Single-layer Spatial Multiplexing with TM9 interference model (User-Specific Reference Symbols) for FDD PCell 1224

8.13.3.4.2 Minimum Requirement Enhanced Performance Requirement Type A – Single-layer Spatial Multiplexing with TM9 interference model (User-Specific Reference Symbols) for TDD PCell 1227

8.13.3.5 Closed-loop spatial multiplexing performance 4Tx Antenna Port for DC 1230

8.13.3.5.1 Minimum Requirement for FDD PCell 1230

8.13.3.5.2 Minimum Requirement for TDD PCell 1232

8.13.3.6 Closed-loop spatial multiplexing performance 4Tx Antenna Port with 256QAM 1234

8.13.3.6.1 Minimum Requirement for FDD PCell 1234

8.13.3.6.2 Minimum Requirement for TDD PCell 1236

8.13.3.7 Closed-loop spatial multiplexing performance 4Tx Antenna Port with Four layers 1237

8.13.3.7.1 Minimum Requirement for FDD PCell 1237

8.13.3.7.2 Minimum Requirement for TDD PCell 1239

8.14 Demodulation (UE supporting Short TTI) 1241

8.14.1 Slot-PDSCH and Subslot-PDSCH 1241

8.14.1.1 FDD (Fixed Reference Channel) 1241

8.14.1.1.1 Open-loop spatial multiplexing performance 1241

8.14.1.1.2 Closed-loop spatial multiplexing performance (User-Specific Reference Signals) 1242

8.14.1.2 TDD (Fixed Reference Channel) 1244

8.14.1.2.1 Open-loop spatial multiplexing performance 1244

8.14.1.2.2 Closed-loop spatial multiplexing performance (User-Specific Reference Signals) 1245

8.14.2 SPDCCH 1246

8.14.2.1 FDD 1246

8.14.2.1.1 Mimimum requirement 1247

8.14.2.2 TDD 1247

8.14.2.2.1 Mimimum requirement 1248

8.15 Demodulation (8 receiver antenna ports) 1249

8.15.1 PDSCH 1249

8.15.1.1 Void 1249

8.15.1.2 TDD (Fixed Reference Channel) 1249

8.15.1.2.1 Transmit diversity performance with 2Tx Antenna Ports (Cell-Specific Reference Symbols) 1249

8.15.1.2.2 Open-loop spatial multiplexing performance with 2Tx Antenna Ports (Cell-Specific Reference Symbols) 1250

8.15.1.2.3 8 Layer Spatial Multiplexing (User-Specific Reference Symbols) 1250

8.15.2 CA 1252

8.15.2.1 Void 1252

8.15.2.2 TDD 1252

8.15.2.2.1 Eight Layer Spatial Multiplexing (User-Specific Reference Symbols) 1252

9 Reporting of Channel State Information 1254

9.1 General 1254

9.1.1 Applicability of requirements 1254

9.1.1.1 Applicability of requirements for different channel bandwidths 1254

9.1.1.2 Applicability and test rules for different CA configurations and bandwidth combination sets 1254

9.1.1.2A Applicability and test rules for different TDD-FDD CA configurations and bandwidth combination sets 1255

9.1.1.3 Test coverage for different number of componenet carriers 1256

9.1.1.4 Applicability of performance requirements for 4Rx capable UEs 1256

9.1.1.4.1 Applicability rule and antenna connection for single carrier tests with 2Rx 1256

9.1.1.4.2 Applicability rule and antenna connection for CA tests with 2Rx 1258

9.1.1.4.3 Applicability rule and antenna connection for single carrier tests with 4Rx 1259

9.1.1.5 Applicability of requirements for UEs supporting coverage enhancement 1259

9.2 CQI reporting definition under AWGN conditions 1259

9.2.1 Minimum requirement PUCCH 1-0 (Cell-Specific Reference Symbols) 1259

9.2.1.1 FDD 1259

9.2.1.2 TDD 1260

9.2.1.3 FDD (CSI measurements in case two CSI subframe sets are configured) 1261

9.2.1.4 TDD (CSI measurements in case two CSI subframe sets are configured) 1264

9.2.1.5 FDD (CSI measurements in case two CSI subframe sets are configured and with CRS assistance information) 1267

9.2.1.6 TDD (CSI measurements in case two CSI subframe sets are configured and with CRS assistance information) 1270

9.2.1.7 FDD (Modulation and TBS index Table 2 and 4-bit CQI Table 2 are used) 1273

9.2.1.8 TDD (Modulation and TBS index Table 2 and 4-bit CQI Table 2 are used) 1274

9.2.1.9 FDD (Modulation and TBS index Table 3 and 4-bit CQI Table 4 are used) 1274

9.2.1.10 TDD (Modulation and TBS index Table 3 and 4-bit CQI Table 4 are used) 1275

9.2.2 Minimum requirement PUCCH 1-1 (Cell-Specific Reference Symbols) 1276

9.2.2.1 FDD 1276

9.2.2.2 TDD 1277

9.2.3 Minimum requirement PUCCH 1-1 (CSI Reference Symbols) 1278

9.2.3.1 FDD 1278

9.2.3.1A FDD (With *channelMeasRestriction* configured) 1279

9.2.3.2 TDD 1280

9.2.3.2A TDD (With *channelMeasRestriction* configured) 1281

9.2.4 Minimum requirement PUCCH 1-1 (With Single CSI Process) 1282

9.2.4.1 FDD 1283

9.2.4.1A FDD (With *interferenceMeasRestriction* configured) 1285

9.2.4.2 TDD 1288

9.2.4.2A TDD (With *interferenceMeasRestriction* configured) 1291

9.2.5 Minimum requirement PUCCH 1-1 (when *csi-SubframeSet –r12* and *EIMTA-MainConfigServCell-r12* are configured) 1294

9.2.6 Minimum requirement PUSCH 3-0 (Cell-Specific Reference Symbols) 1297

9.2.6.1 Frame structure type 3 with FDD Pcell 1297

9.2.6.2 Frame structure type 3 with TDD Pcell 1299

9.2.7 Minimum requirement PUSCH 3-1 (CSI Reference Symbol) 1301

9.2.7.1 Frame structure type 3 wth FDD Pcell 1301

9.2.7.2 Frame structure type 3 wth TDD Pcell 1303

9.3 CQI reporting under fading conditions 1307

9.3.1 Frequency-selective scheduling mode 1307

9.3.1.1 Minimum requirement PUSCH 3-0 (Cell-Specific Reference Symbols) 1307

9.3.1.1.1 FDD 1307

9.3.1.1.2 TDD 1308

9.3.1.1.3 FDD (CSI measurements in case two CSI subframe sets are configured and with CRS assistance information) 1309

9.3.1.1.4 TDD (CSI measurements in case two CSI subframe sets are configured and with CRS assistance information) 1313

9.3.1.1.5 TDD (when *csi-SubframeSet –r12* is configured) 1316

9.3.1.2 Minimum requirement PUSCH 3-1 (CSI Reference Symbol) 1318

9.3.1.2.1 FDD 1318

9.3.1.2.2 TDD 1319

9.3.1.2.3 FDD (Modulation and TBS index Table 2 and 4-bit CQI Table 2 are used) 1321

9.3.1.2.4 TDD (Modulation and TBS index Table 2 and 4-bit CQI Table 2 are used) 1322

9.3.1.2.5 Void 1323

9.3.1.2.6 TDD (when *csi-SubframeSet –r12* is configured with one CSI process) 1323

9.3.2 Frequency non-selective scheduling mode 1327

9.3.2.1 Minimum requirement PUCCH 1-0 (Cell-Specific Reference Symbol) 1327

9.3.2.1.1 FDD 1327

9.3.2.1.2 TDD 1329

9.3.2.2 Minimum requirement PUCCH 1-1 (CSI Reference Symbol) 1331

9.3.2.2.1 FDD 1331

9.3.2.2.2 TDD 1332

9.3.3 Frequency-selective interference 1334

9.3.3.1 Minimum requirement PUSCH 3-0 (Cell-Specific Reference Symbol) 1334

9.3.3.1.1 FDD 1334

9.3.3.1.2 TDD 1335

9.3.3.2 Void 1336

9.3.3.2.1 Void 1336

9.3.3.2.2 Void 1336

9.3.4 UE-selected subband CQI 1336

9.3.4.1 Minimum requirement PUSCH 2-0 (Cell-Specific Reference Symbols) 1336

9.3.4.1.1 FDD 1336

9.3.4.1.2 TDD 1337

9.3.4.2 Minimum requirement PUCCH 2-0 (Cell-Specific Reference Symbols) 1338

9.3.4.2.1 FDD 1338

9.3.4.2.2 TDD 1339

9.3.5 Additional requirements for enhanced receiver Type A 1342

9.3.5.1 Minimum requirement PUCCH 1-0 (Cell-Specific Reference Symbol) 1342

9.3.5.1.1 FDD 1342

9.3.5.1.2 TDD 1343

9.3.5.2 Minimum requirement PUCCH 1-1 (CSI Reference Symbol) 1345

9.3.5.2.1 FDD 1345

9.3.5.2.2 TDD 1348

9.3.6 Minimum requirement (With multiple CSI processes) 1351

9.3.6.1 FDD 1351

9.3.6.2 TDD 1356

9.3.7 Minimum requirement PUSCH 3-2 1360

9.3.7.1 FDD 1360

9.3.7.2 TDD 1361

9.3.8 Additional requirements for enhanced receiver Type B 1363

9.3.8.1 Minimum requirement PUCCH 1-1 (Cell-Specific Reference Symbols) 1363

9.3.8.1.1 FDD 1363

9.3.8.1.2 TDD 1364

9.3.8.2 Minimum requirement PUCCH 1-1 (CSI Reference Symbols) 1366

9.3.8.2.1 FDD 1366

9.3.8.2.2 TDD 1368

9.3.8.3 Minimum requirement with CSI process 1371

9.3.8.3.1 FDD 1371

9.3.8.3.2 TDD 1374

9.4 Reporting of Precoding Matrix Indicator (PMI) 1377

9.4.1 Single PMI 1378

9.4.1.1 Minimum requirement PUSCH 3-1 (Cell-Specific Reference Symbols) 1378

9.4.1.1.1 FDD 1378

9.4.1.1.2 TDD 1379

9.4.1.2 Minimum requirement PUCCH 2-1 (Cell-Specific Reference Symbols) 1380

9.4.1.2.1 FDD 1380

9.4.1.2.2 TDD 1382

9.4.1.3 Minimum requirement PUSCH 3-1 (CSI Reference Symbol) 1383

9.4.1.3.1 FDD 1383

9.4.1.3.2 TDD 1386

9.4.1.3.3 FDD (with Class A 12Tx codebook) 1389

9.4.1.3.4 TDD (with Class A 12Tx codebook) 1391

9.4.1.3.5 FDD (with Class A 24Tx codebook) 1394

9.4.1.3.6 TDD (with Class A 24Tx codebook) 1396

9.4.1.4 Minimum requirement PUCCH 1-1 (CSI Reference Symbol) 1399

9.4.1.4.1 FDD (with 4Tx enhanced codebook) 1399

9.4.1.4.2 TDD (with 4Tx enhanced codebook) 1401

9.4.1.4.3 FDD (with Class B alternative codebook for one CSI-RS resource configured) 1404

9.4.1.4.4 TDD (with Class B alternative codebook for one CSI-RS resource configured) 1406

9.4.1a Void 1409

9.4.1a.1 Void 1409

9.4.1a.1.1 Void 1409

9.4.1a.1.2 Void 1409

9.4.2 Multiple PMI 1409

9.4.2.1 Minimum requirement PUSCH 1-2 (Cell-Specific Reference Symbols) 1409

9.4.2.1.1 FDD 1409

9.4.2.1.2 TDD 1410

9.4.2.2 Minimum requirement PUSCH 2-2 (Cell-Specific Reference Symbols) 1411

9.4.2.2.1 FDD 1411

9.4.2.2.2 TDD 1412

9.4.2.3 Minimum requirement PUSCH 1-2 (CSI Reference Symbol) 1413

9.4.2.3.1 FDD 1413

9.4.2.3.2 TDD 1415

9.4.2.3.3 FDD (with 4Tx enhanced codebook) 1418

9.4.2.3.4 TDD (with 4Tx enhanced codebook) 1420

9.4.2.3.5 FDD (with Class A 16Tx codebook) 1422

9.4.2.3.6 TDD (with Class A 16Tx codebook) 1425

9.4.2.3.7 FDD (with Class A 32Tx codebook) 1428

9.4.2.3.8 TDD (with Class A 32Tx codebook) 1431

9.4.2.3.9 FDD (with Class A 16Tx advanced codebook) 1434

9.4.2.3.10 TDD (with Class A 16Tx advanced codebook) 1437

9.4.3 Void 1440

9.5 Reporting of Rank Indicator (RI) 1440

9.5.1 Minimum requirement (Cell-Specific Reference Symbols) 1440

9.5.1.1 FDD 1440

9.5.1.2 TDD 1441

9.5.2 Minimum requirement (CSI Reference Symbols) 1442

9.5.2.1 FDD 1442

9.5.2.2 TDD 1444

9.5.3 Minimum requirement (CSI measurements in case two CSI subframe sets are configured) 1446

9.5.3.1 FDD 1446

9.5.3.2 TDD 1449

9.5.4 Minimum requirement (CSI measurements in case two CSI subframe sets are configured and CRS assistance information are configured) 1452

9.5.4.1 FDD 1452

9.5.4.2 TDD 1455

9.5.5 Minimum requirement (with CSI process) 1458

9.5.5.1 FDD 1459

9.5.5.2 TDD 1462

9.6 Additional requirements for carrier aggregation 1465

9.6.1 Periodic reporting on multiple cells (Cell-Specific Reference Symbols) 1465

9.6.1.1 FDD 1465

9.6.1.2 TDD 1471

9.6.1.3 TDD-FDD CA with FDD PCell 1477

9.6.1.4 TDD-FDD CA with TDD PCell 1482

9.7 CSI reporting (Single receiver antenna) 1488

9.7.1 CQI reporting definition under AWGN conditions 1489

9.7.1.1 FDD and half-duplex FDD 1489

9.7.1.2 TDD 1489

9.7.1.3 FDD (Category 1bis UE) 1490

9.7.1.4 TDD (Category 1bis UE) 1491

9.7.2 CQI reporting under fading conditions 1492

9.7.2.1 FDD and half-duplex FDD 1492

9.7.2.2 TDD 1493

9.7.2.3 FDD (Category 1bis UE) 1494

9.7.2.4 TDD (Category 1bis UE) 1495

9.8 CSI reporting (UE supporting coverage enhancement) 1496

9.8.1 CQI reporting definition under AWGN conditions 1496

9.8.1.1 FDD and half-duplex FDD 1496

9.8.1.2 TDD 1497

9.8.2 UE-selected subband CQI 1498

9.8.2.1 FDD and half-duplex FDD 1498

9.8.2.2 TDD 1502

9.8.3 CQI reporting definition for UE supporting 64QAM under AWGN 1505

9.8.3.1 FDD and half-duplex FDD 1505

9.8.3.2 TDD 1506

9.8.4 CQI reporting definition for UE supporting alternative table under AWGN 1507

9.8.4.1 FDD and half-duplex FDD 1507

9.8.4.2 TDD 1508

9.8.5 PMI reporting with PUCCH 1-1 (CSI Reference Symbol) 1509

9.8.5.1 FDD 1510

9.8.5.2 TDD 1511

9.9 CSI reporting for 4Rx UE 1512

9.9.1 CQI reporting definition under AWGN conditions 1512

9.9.1.1 Minimum requirement PUCCH 1-0 with Rank 1 (Cell-Specific Reference Symbols) 1513

9.9.1.1.1 FDD 1513

9.9.1.1.2 TDD 1513

9.9.1.2 Minimum requirement PUCCH 1-1 with Rank 2 (CSI Reference Symbols) 1514

9.9.1.2.1 FDD 1514

9.9.1.2.2 TDD 1515

9.9.1.3 Minimum requirement PUCCH 1-1 with Rank 4 (Cell-Specific Reference Symbols) 1516

9.9.1.3.1 FDD 1517

9.9.1.3.2 TDD 1517

9.9.1.4 Minimum requirement PUCCH 1-1 with Rank 3 (CSI Reference Symbols) 1518

9.9.1.4.1 FDD 1518

9.9.1.4.2 TDD 1519

9.9.2 CQI reporting definition under fading conditions 1520

9.9.2.1 Minimum requirement PUCCH 1-0 (Cell-Specific Reference Symbol) for enhanced receiver Type A 1520

9.9.2.1.1 FDD 1521

9.9.2.1.2 TDD 1522

9.9.2.2 Minimum requirement PUCCH 1-1 (CSI Reference Symbol) for enhanced receiver Type A 1524

9.9.2.2.1 FDD 1524

9.9.2.2.2 TDD 1527

9.9.3 Reporting of Precoding Matrix Indicator (PMI) for 4Rx UE 1530

9.9.3.1 Minimum requirement PUSCH 3-1 (CSI Reference Symbol) 1531

9.9.3.1.1 TDD 1531

9.9.4 Reporting of Rank Indicator (RI) 1533

9.9.4.1 Minimum requirement (Cell-Specific Reference Symbols) 1533

9.9.4.1.1 FDD 1533

9.9.4.1.2 TDD 1535

9.9.4.2 Minimum requirement (CSI Reference Symbols) 1536

9.9.4.2.1 FDD 1536

9.9.4.2.2 TDD 1538

9.10 Reporting of CSI-RS Resource Indicator (CRI) 1540

9.10.1 Minimum requirement (PUSCH 3-1) 1541

9.10.1.1 FDD 1541

9.10.1.2 TDD 1543

9.10.2 Minimum requirement (PUSCH 3-1, QCL Type C) 1545

9.10.2.1 FDD 1545

9.10.2.2 TDD 1548

9.11 Reporting of Hybrid Channel state information 1551

9.11.1 Minimum requirement (with eMIMO-Type configured as Class B with more than one CSI-RS resource configured and eMIMO-Type2 as Class B with one CSI-RS resource configured) 1551

9.11.1.1 FDD 1552

9.11.1.2 TDD 1554

9.12 CSI reporting (UE supporting Short TTI) 1556

9.12.1 CQI reporting under fading conditions (Cell-Specific Reference Symbol) 1556

9.12.1.1 FDD 1556

9.12.1.2 TDD 1559

9.12.2 CQI reporting under fading conditions (CSI Reference Symbol) 1560

9.12.2.1 FDD 1560

9.12.2.2 TDD 1563

9.13 CSI reporting for 8Rx UE 1565

9.13.1 CQI reporting definition under AWGN conditions 1565

9.13.1.1 Minimum requirement PUCCH 1-1 with Rank 4 (CSI Reference Symbols) 1565

9.13.1.2.1 Void 1565

9.13.1.2.2 TDD 1565

10 Performance requirement (MBMS) 1566

10.1 FDD (Fixed Reference Channel) 1566

10.1.1 Minimum requirement 1567

10.2 TDD (Fixed Reference Channel) 1568

10.2.1 Minimum requirement 1568

10.3 FDD (Fixed Reference Channel) with FeMBMS 1569

10.3.1 Minimum requirement for FeMBMS Unicast-mixed Cell under CA 1569

10.3.1.1 Minimum requirement with 1.25kHz subcarrier spacing 1569

10.3.1.2 Minimum requirement with 7.5kHz subcarrier spacing 1570

10.3.2 Minimum requirement for FeMBMS Unicast-mixed Cell as Non-Serving Cell 1571

10.3.2.1 Minimum requirement with 1.25kHz subcarrier spacing 1571

10.3.2.2 Minimum requirement with 7.5kHz subcarrier spacing 1572

10.3.3 Minimum requirement for MBMS Dedicated cell 1573

10.3.3.1 Minimum requirement with 1.25kHz subcarrier spacing 1573

10.3.3.2 Minimum requirement with 7.5kHz subcarrier spacing 1574

10.3.3.3 Minimum requirement with 15kHz subcarrier spacing 1575

10.4 FDD with 5G terrestrial broadcast 1576

10.4.1 Minimum requirement for PMCH decoding 1576

10.4.1.1 Minimum requirement with 0.37kHz subcarrier spacing 1576

10.4.1.2 Minimum requirement with 2.5kHz subcarrier spacing 1577

10.4.2 Minimum requirement for CAS detection 1578

10.4.2.1 Minimum requirement for PBCH detection 1578

11 Performance requirement (ProSe Direct Discovery) 1578

11.1 General 1579

11.1.1 Applicability of requirements 1579

11.1.2 Reference DRX configuration 1579

11.2 Demodulation of PSDCH (single link performance) 1579

11.2.1 FDD (in-coverage) 1579

11.2.2 TDD (in-coverage) 1580

11.2.3 FDD (out-of-coverage) 1581

11.3 Power imbalance performance with two links 1582

11.3.1 FDD 1582

11.3.2 TDD 1583

11.4 Multiple timing reference test 1584

11.4.1 FDD 1585

11.5 Maximum Sidelink processes test 1586

11.5.1 FDD 1586

11.5.2 TDD 1587

12 Performance requirement (ProSe Direct Communication) 1589

12.1 General 1589

12.1.1 Applicability of requirements 1589

12.1.1.1 Applicability of requirements for different channel bandwidths 1589

12.1.1.2 Test coverage for different number of component carriers 1589

12.1.1.3 Applicability and test rules for different CA configurations and bandwidth combination sets 1589

12.1.2 Reference DRX configuration 1590

12.2 Demodulation of PSSCH 1590

12.2.1 FDD 1590

12.3 Demodulation of PSCCH 1591

12.3.1 FDD 1592

12.4 Demodulation of PSBCH 1593

12.4.1 FDD 1593

12.5 Power imbalance performance with two links 1593

12.5.1 FDD 1593

12.6 Multiple timing reference test 1595

12.6.1 FDD 1595

12.7 Maximum Sidelink processes test 1598

12.7.1 FDD 1598

12.8 Sustained downlink data rate with active Sidelink 1599

13 Void 1601

14 Performance requirement (V2X Sidelink Communication) 1601

14.1 General 1601

14.1.1 Applicability of requirements 1601

14.2 Demodulation of PSSCH 1602

14.3 Demodulation of PSCCH 1603

14.4 Power imbalance performance with two links 1603

14.5 Demodulation of PSBCH 1604

14.6 Demodulation of PSSCH with eNB based synchronization 1605

14.7 Soft buffer test 1605

14.8 PSCCH decoding capability test 1606

14.9 Sustained downlink data rate with active sidelink 1607

14.10 Soft buffer test (CA) 1608

14.11 PSCCH/PSSCH decoding capability test (CA) 1609

Annex A (normative): Measurement channels 1614

A.1 General 1614

A.2 UL reference measurement channels 1614

A.2.1 General 1614

A.2.1.1 Applicability and common parameters 1614

A.2.1.2 Determination of payload size 1614

A.2.1.3 Overview of UL reference measurement channels 1615

A.2.2 Reference measurement channels for FDD 1638

A.2.2.1 Full RB allocation 1638

A.2.2.1.1 QPSK 1638

A.2.2.1.2 16-QAM 1640

A.2.2.1.3 64-QAM 1642

A.2.2.1.4 256 QAM 1643

A.2.2.2 Partial RB allocation 1643

A.2.2.2.1 QPSK 1644

A.2.2.2.2 16-QAM 1647

A.2.2.2.3 64-QAM 1649

A.2.2.2.4 256 QAM 1651

A.2.2.3 Void 1651

A.2.2.4 subPRB allocation 1652

A.2.3 Reference measurement channels for TDD 1652

A.2.3.1 Full RB allocation 1652

A.2.3.1.1 QPSK 1652

A.2.3.1.2 16-QAM 1655

A.2.3.1.3 64-QAM 1658

A.2.3.1.4 256 QAM 1658

A.2.3.2 Partial RB allocation 1658

A.2.3.2.1 QPSK 1659

A.2.3.2.2 16-QAM 1663

A.2.3.2.3 64-QAM 1668

A.2.3.2.4 256 QAM 1670

A.2.3.3 Void 1670

A.2.3.4 subPRB allocation 1671

A.2.4 Reference measurement channels for UE category NB1 1671

A.2.5 Reference measurement channels for LAA 1672

A.2.5.1 Full RB allocation 1672

A.2.5.1.1 QPSK 1672

A.2.5.1.2 16QAM 1673

A.2.5.1.3 64QAM 1673

A.2.5.2 Partial RB allocation 1673

A.2.5.2.1 QPSK 1674

A.2.5.2.2 16QAM 1674

A.2.5.2.3 64QAM 1675

A.3 DL reference measurement channels 1675

A.3.1 General 1675

A.3.1.1 Overview of DL reference measurement channels 1676

A.3.2 Reference measurement channel for receiver characteristics 1701

A.3.3 Reference measurement channels for PDSCH performance requirements (FDD) 1731

A.3.3.1 Single-antenna transmission (Common Reference Symbols) 1731

A.3.3.2 Multi-antenna transmission (Common Reference Symbols) 1736

A.3.3.2.1 Two antenna ports 1736

A.3.3.2.2 Four antenna ports 1744

A.3.3.3 Reference Measurement Channel for UE-Specific Reference Symbols 1749

A.3.3.3.0 Two antenna ports (no CSI-RS) 1749

A.3.3.3.1 Two antenna port (CSI-RS) 1750

A.3.3.3.2 Four antenna ports (CSI-RS) 1753

A.3.3.3.2A Eight antenna ports (CSI-RS) 1760

A.3.3.3.3 Twelve antenna port (CSI-RS) 1762

A.3.3.3.4 Sixteen antenna port (CSI-RS) 1763

A.3.3.3.5 Twenty-four antenna port (CSI-RS) 1764

A.3.3.3.6 Thirty-two antenna port (CSI-RS) 1765

A.3.4 Reference measurement channels for PDSCH performance requirements (TDD) 1767

A.3.4.1 Single-antenna transmission (Common Reference Symbols) 1767

A.3.4.2 Multi-antenna transmission (Common Reference Signals) 1775

A.3.4.2.1 Two antenna ports 1775

A.3.4.2.2 Four antenna ports 1788

A.3.4.3 Reference Measurement Channels for UE-Specific Reference Symbols 1795

A.3.4.3.1 Single antenna port (Cell Specific) 1795

A.3.4.3.2 Two antenna ports (Cell Specific) 1796

A.3.4.3.3 Two antenna ports (CSI-RS) 1798

A.3.4.3.4 Four antenna ports (CSI-RS) 1806

A.3.4.3.5 Eight antenna ports (CSI-RS) 1813

A.3.4.3.6 Twelve antenna ports (CSI-RS) 1819

A.3.4.3.7 Sixteen antenna ports (CSI-RS) 1820

A.3.4.3.8 Twenty-four antenna ports (CSI-RS) 1821

A.3.4.3.9 Thirty-two antenna ports (CSI-RS) 1822

A.3.5 Reference measurement channels for PDCCH/PCFICH performance requirements 1824

A.3.5.1 FDD 1824

A.3.5.2 TDD 1824

A.3.5.3 LAA 1825

A.3.6 Reference measurement channels for PHICH performance requirements 1825

A.3.7 Reference measurement channels for PBCH performance requirements 1825

A.3.8 Reference measurement channels for MBMS performance requirements 1826

A.3.8.1 FDD 1826

A.3.8.2 TDD 1831

A.3.9 Reference measurement channels for sustained downlink data rate provided by lower layers 1833

A.3.9.1 FDD 1833

A.3.9.2 TDD 1837

A.3.9.3 FDD (EPDCCH scheduling) 1851

A.3.9.4 TDD (EPDCCH scheduling) 1852

A.3.9.5 LAA 1854

A.3.10 Reference Measurement Channels for EPDCCH performance requirements 1856

A.3.10.1 FDD 1856

A.3.10.2 TDD 1856

A.3.11 Reference Measurement Channels for MPDCCH performance requirements 1856

A.3.11.1 FDD and half-duplex FDD 1856

A.3.11.2 TDD 1857

A.3.12 Reference measurement channels for NPDSCH performance requirements 1858

A.3.12.1 In-band 1858

A.3.12.1.2 Two-antenna transmission 1858

A.3.12.2 Standalone/Guard-band 1860

A.3.12.2.1 Single-antenna transmission 1860

A.3.13 Reference measurement channels for NPDCCH performance requirements 1863

A.3.13.1 Half-duplex FDD 1863

A.3.13.2 TDD 1864

A.3.14 Reference measurement channels for NPBCH performance requirements for Cat NB1 UEs 1864

A.3.15 Reference Measurement Channels for LAA SCell with frame structure Type-3 1865

A.3.15.1 Multi-antenna transmission (Common Reference Symbols) 1865

A.3.15.1.1 Four antenna ports 1865

A.3.15.2 Reference Measurement Channel for UE-Specific Reference Symbols 1865

A.3.15.2.1 Two antenna ports (CSI-RS) 1865

A.3.16 Reference measurement channels for Slot-PDSCH and Subslot-PDSCH performance requirements 1867

A.3.16.1 FDD 1867

A.3.16.2 TDD 1871

A.3.17 Reference measurement channels for SPDCCH performance requirements 1872

A.3.17.1 FDD 1872

A.3.17.2 TDD 1873

A.4 CSI reference measurement channels 1873

A.5 OFDMA Channel Noise Generator (OCNG) 1888

A.5.1 OCNG Patterns for FDD 1888

A.5.1.1 OCNG FDD pattern 1: One sided dynamic OCNG FDD pattern 1888

A.5.1.2 OCNG FDD pattern 2: Two sided dynamic OCNG FDD pattern 1889

A.5.1.3 OCNG FDD pattern 3: 49 RB OCNG allocation with MBSFN in 10 MHz 1889

A.5.1.3A OCNG FDD pattern 3A: 49 RB OCNG allocation with MBSFN enhancement in 10 MHz 1890

A.5.1.4 OCNG FDD pattern 4: One sided dynamic OCNG FDD pattern for MBMS transmission 1890

A.5.1.4A OCNG FDD pattern 4A: One sided dynamic OCNG FDD pattern for enhanced MBMS transmission 1891

A.5.1.5 OCNG FDD pattern 5: One sided dynamic 16QAM modulated OCNG FDD pattern 1892

A.5.1.6 OCNG FDD pattern 6: dynamic OCNG FDD pattern when user data is in 2 non-contiguous blocks 1893

A.5.1.8 OCNG FDD pattern 8: Dynamic OCNG FDD pattern for TM10 transmission 1894

A.5.2 OCNG Patterns for TDD 1895

A.5.2.1 OCNG TDD pattern 1: One sided dynamic OCNG TDD pattern 1895

A.5.2.2 OCNG TDD pattern 2: Two sided dynamic OCNG TDD pattern 1896

A.5.2.3 OCNG TDD pattern 3: 49 RB OCNG allocation with MBSFN in 10 MHz 1897

A.5.2.4 OCNG TDD pattern 4: One sided dynamic OCNG TDD pattern for MBMS transmission 1897

A.5.2.5 OCNG TDD pattern 5: One sided dynamic 16QAM modulated OCNG TDD pattern 1898

A.5.2.6 OCNG TDD pattern 6: dynamic OCNG TDD pattern when user data is in 2 non-contiguous blocks 1899

A.5.2.8 OCNG TDD pattern 8: Dynamic OCNG TDD pattern for TM10 transmission 1900

A.5.3 OCNG Patterns for Narrowband IoT 1901

A.5.3.1 Narrowband IoT OCNG pattern 1 1901

A.5.4 OCNG Patterns for frame structure type 3 1902

A.5.4.1 OCNG FS3 pattern 1: One sided dynamic OCNG frame structure type 3 pattern 1902

A.5.4.2 OCNG FS3 pattern 2: Two sided dynamic OCNG frame structure 3 pattern 1903

A.6 Sidelink reference measurement channels 1904

A.6.1 General 1904

A.6.1.1 Overview of ProSe reference measurement channels 1904

A.6.2 Reference measurement channel for receiver characteristics 1905

A.6.3 Reference measurement channels for PSDCH performance requirements 1907

A.6.4 Reference measurement channels for PSCCH performance requirements 1908

A.6.5 Reference measurement channels for PSSCH performance requirements 1908

A.6.6 Reference measurement channels for PSBCH performance requirements 1909

A.7 Sidelink reference resource pool configurations 1910

A.7.1 Reference resource pool configurations for ProSe Direct Discovery demodulation tests 1910

A.7.1.1 FDD 1910

A.7.1.2 TDD 1913

A.7.2 Reference resource pool configurations for ProSe Direct Communication demodulation tests 1915

A.7.2.1 FDD 1915

A.8 V2X reference measurement channels 1920

A.8.1 General 1920

A.8.1.1 Overview of V2X reference measurement channels 1921

A.8.2 Reference measurement channel for receiver characteristics 1921

A.8.3 Reference measurement channel for transmitter characteristics 1923

A.8.4 Reference measurement for PSCCH performance requirements 1926

A.8.5 Reference measurement for PSSCH performance requirements 1927

A.8.6 Reference measurement for PSBCH performance requirements 1927

A.9 V2X reference resource pool configurations 1928

Annex B (normative): Propagation conditions 1931

B.1 Static propagation condition 1931

B.1.1 UE Receiver with 2Rx 1931

B.1.2 UE Receiver with 4Rx 1931

B.1.3 UE Receiver with 8Rx 1932

B.2 Multi-path fading propagation conditions 1933

B.2.1 Delay profiles 1933

B.2.2 Combinations of channel model parameters 1934

B.2.3 MIMO Channel Correlation Matrices 1935

B.2.3.1 Definition of MIMO Correlation Matrices 1935

B.2.3.2 MIMO Correlation Matrices at High, Medium and Low Level 1941

B.2.3A MIMO Channel Correlation Matrices using cross polarized antennas 1944

B.2.3A.1 Definition of MIMO Correlation Matrices using cross polarized antennas 1945

B.2.3A.2 Spatial Correlation Matrices using cross polarized antennas at eNB and UE sides 1945

B.2.3A.2.1 Spatial Correlation Matrices at eNB side 1945

B.2.3A.2.2 Spatial Correlation Matrices at UE side 1946

B.2.3A.4 Beam steering approach 1949

B.2.3B MIMO Channel Correlation Matrices using two-dimension cross polarized antennas at eNB and cross polarized antennas at UE 1949

B.2.3B.1 Definition of MIMO Correlation Matrices using two-dimension cross polarized antennas at eNB and cross polarized antennas at UE 1950

B.2.3B.2 Spatial Correlation Matrices using two-dimension cross polarized antennas at eNB and cross polarized antennas at UE 1951

B.2.3B.2.1 Spatial Correlation Matrices at eNB side 1951

B.2.3B.2.2 Spatial Correlation Matrices at UE side 1951

B.2.3B.3 MIMO Correlation Matrices using two-dimension cross polarized antennas at eNB and cross polarized antennas at UE 1951

B.2.3B.4 Beam steering approach 1954

B.2.3B.4A Beam steering approach with dual cluster beams 1955

B.2.4 Propagation conditions for CQI tests 1956

B.2.4.1 Propagation conditions for CQI tests with multiple CSI processes 1956

B.2.5 Void 1956

B.2.6 MBSFN Propagation Channel Profile 1956

B.2.6.1 Subcarrier spacing 15kHz or 7.5kHz 1956

B.2.6.2 Subcarrier spacing 1.25kHz 1957

B.2.6.3 Subcarrier spacing 0.37kHz 1958

B.2.6.4 Subcarrier spacing 2.5kHz 1958

B.3 High speed train scenario 1959

B.3A HST-SFN scenario 1960

B.3B HST-SFN scenario for 500 km/h speed 1964

B.3C HST scenario for 500 km/h speed 1964

B.4 Beamforming Model 1964

B.4.1 Single-layer random beamforming (Antenna port 5, 7, or 8) 1964

B.4.1A Single-layer random beamforming (Antenna port 7, 8, 11 or 13 with enhanced DMRS table configured) 1965

B.4.2 Dual-layer random beamforming (antenna ports 7 and 8) 1965

B.4.3 Generic beamforming model (antenna ports 7-14) 1966

B.4.4 Random beamforming for EPDCCH distributed transmission (Antenna port 107 and 109) 1966

B.4.5 Random beamforming for EPDCCH localized transmission (Antenna port 107, 108, 109 or 110) 1967

B.4.6 Beamforming model for CRI test 1967

B.5 Interference models for enhanced performance requirements Type-A 1968

B.5.1 Dominant interferer proportion 1968

B.5.2 Transmission mode 3 interference model 1969

B.5.3 Transmission mode 4 interference model 1969

B.5.4 Transmission mode 9 interference model 1970

B.6 Interference models for enhanced performance requirements Type-B 1970

B.6.1 Transmission mode 2 interference model 1970

B.6.2 Transmission mode 3 interference model 1970

B.6.3 Transmission mode 4 interference model 1971

B.6.4 Transmission mode 9 interference model 1971

B.6.5 CRS interference model 1972

B.6.6 Random interference model 1972

B.7 Interference models for enhanced downlink control channel performance requirements Type A and B 1973

B.7.1 PDCCH, PCFICH and PHICH interference model 1973

B.8 Burst transmission models for Frame structure type 3 1974

B.8.1 Burst transmission model for one LAA SCell 1974

B.8.2 Burst transmission model for multiple LAA SCell(s) 1974

Annex C (normative): Downlink Physical Channels 1976

C.1 General 1976

C.2 Set-up 1976

C.3 Connection 1976

C.3.1 Measurement of Receiver Characteristics 1976

C.3.2 Measurement of Performance requirements 1977

C.3.3 Aggressor cell power allocation for Measurement of Performance Requirements when ABS is Configured 1978

C.3.4 Power Allocation for Measurement of Performance Requirements when Quasi Co-location Type B: same Cell ID 1979

C.3.5 Simplified CA testing method 1979

C.3.6 Measurement of Receiver Characteristics for Narrowband IoT 1980

Annex D (normative): Characteristics of the interfering signal 1981

D.1 General 1981

D.2 Interference signals 1981

Annex E (normative): Environmental conditions 1982

E.1 General 1982

E.2 Environmental 1982

E.2.1 Temperature 1982

E.2.2 Voltage 1982

E.2.3 Vibration 1983

Annex F (normative): Transmit modulation 1984

F.1 Measurement Point 1984

F.2 Basic Error Vector Magnitude measurement 1984

F.3 Basic in-band emissions measurement 1985

F.4 Modified signal under test 1985

F.5 Window length 1987

F.5.1 Timing offset 1987

F.5.2 Window length 1987

F.5.3 Window length for normal CP 1987

F.5.4 Window length for Extended CP 1988

F.5.5 Window length for PRACH 1988

F.5.F Window length for category NB1 1989

F.6 Averaged EVM 1989

F.6.F Averaged EVM for category NB1 1990

F.7 Spectrum Flatness 1990

Annex G (informative): Reference sensitivity level in lower SNR 1991

G.1 General 1991

G.2 Typical receiver sensitivity performance (QPSK) 1991

G.3 Reference measurement channel for REFSENSE in lower SNR 1997

Annex H (normative): Modified MPR behavior 2000

H.1 Indication of modified MPR behavior 2000

Annex I (normative): Supported Post Antenna Gain 2001

I.1 Declared Supported Post Antenna Gain for UE 2001

Annex J (informative): Change history 2002