3GPP TS 38.101-3 V15.20.0 (2022-12)

Technical Specification

3rd Generation Partnership Project;

Technical Specification Group Radio Access Network;

NR;

User Equipment (UE) radio transmission and reception;

Part 3: Range 1 and Range 2 Interworking operation with other radios

(Release 15)

** 

The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP..  
The present document has not been subject to any approval process by the 3GPPOrganizational Partners and shall not be implemented.  
This Specification is provided for future development work within 3GPPonly. The Organizational Partners accept no liability for any use of this Specification.  
Specifications and Reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organizational Partners' Publications Offices.

***3GPP***

Postal address

3GPP support office address

650 Route des Lucioles - Sophia Antipolis

Valbonne - FRANCE

Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16

Internet

http://www.3gpp.org

***Copyright Notification***

No part may be reproduced except as authorized by written permission.  
The copyright and the foregoing restriction extend to reproduction in all media.

© 2022, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

UMTS™ is a Trade Mark of ETSI registered for the benefit of its members

3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  
LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners

GSM® and the GSM logo are registered and owned by the GSM Association

Contents

Foreword 11

1 Scope 12

2 References 12

3 Definitions, symbols and abbreviations 13

3.1 Definitions 13

3.2 Symbols 13

3.3 Abbreviations 13

4 General 14

4.1 Relationship between minimum requirements and test requirements 14

4.2 Applicability of minimum requirements 14

4.3 Specification suffix information 15

5 Operating bands and channel arrangement 16

5.1 General 16

5.2 Operating bands 16

5.2A Operating bands for CA 16

5.2A.1 Inter-band CA between FR1 and FR2 16

5.2B Operating bands for DC 17

5.2B.1 General 17

5.2B.2 Void 17

5.2B.3 Void 17

5.2B.4 Void 17

5.2B.5 Void 17

5.2B.6 Void 17

5.2B.7 Void 17

5.3 UE Channel bandwidth 17

5.3A UE Channel bandwidth for CA 17

5.3A.1 Inter-band CA between FR1 and FR2 17

5.3B UE Channel bandwidth for EN-DC 17

5.3B.1 Intra-band EN-DC in FR1 18

5.3B.1.1 General 18

5.3B.1.2 BCS for Intra-band contiguous EN-DC 18

5.3B.1.3 BCS for Intra-band non-contiguous EN-DC 19

5.4 Void 20

5.4A Channel arrangement for CA 20

5.4B Channel arrangement for DC 20

5.4B.1 Channel spacing for intra-band EN-DC carriers 20

5.5 Configuration 21

5.5A Configuration for CA 21

5.5A.1 Inter-band CA configurations between FR1 and FR2 21

5.5B Configuration for DC 24

5.5B.1 General 24

5.5B.2 Intra-band contiguous EN-DC 24

5.5B.3 Intra-band non-contiguous EN-DC 25

5.5B.4 Inter-band EN-DC within FR1 25

5.5B.4.1 Inter-band EN-DC configurations within FR1 (two bands) 25

5.5B.4.2 Inter-band EN-DC configurations within FR1 (three bands) 28

5.5B.4.3 Inter-band EN-DC configurations within FR1 (four bands) 33

5.5B.4.4 Inter-band EN-DC configurations within FR1 (five bands) 37

5.5B.4.5 Inter-band EN-DC configurations within FR1 (six bands) 39

5.5B.4a Inter-band NE-DC within FR1 39

5.5B.4a.1 Inter-band NE-DC configurations within FR1 (two bands) 39

5.5B.5 Inter-band EN-DC including FR2 39

5.5B.5.1 Inter-band EN-DC configurations including FR2 (two bands) 39

5.5B.5.2 Inter-band EN-DC configurations including FR2 (three bands) 43

5.5B.5.3 Inter-band EN-DC configurations including FR2 (four bands) 46

5.5B.5.4 Inter-band EN-DC configurations including FR2 (five bands) 48

5.5B.5.5 Void 49

5.5B.6 Inter-band EN-DC including FR1 and FR2 49

5.5B.6.1 Void 49

5.5B.6.2 Inter-band EN-DC configurations including FR1 and FR2 (three bands) 49

5.5B.6.3 Inter-band EN-DC configurations including FR1 and FR2 (four bands) 51

5.5B.6.4 Inter-band EN-DC configurations including FR1 and FR2 (five bands) 52

5.5B.6.5 Inter-band EN-DC configurations including FR1 and FR2 (six bands) 53

5.5B.7 Inter-band NR-DC between FR1 and FR2 53

5.5B.7.0 General 53

5.5B.7.1 Inter-band NR-DC configurations between FR1 and FR2 (two bands) 53

6 Transmitter characteristics 54

6.1 General 54

6.2 Void 54

6.2A Transmitter power for CA 54

6.2A.1 UE maximum output power for CA 54

6.2A.1.1 Inter-band CA between FR1 and FR2 54

6.2A.2 UE maximum output power reduction for CA 54

6.2A.2.1 Inter-band CA between FR1 and FR2 54

6.2A.3 UE additional maximum output power reduction for CA 54

6.2A.4 Configured output power for CA 54

6.2A.4.1 Configured output power level 54

6.2A.4.2 ΔTIB,c for CA 55

6.2A.4.2.1 ΔTIB,c for Inter-band CA between FR1 and FR2 55

6.2B Transmitter power for DC 55

6.2B.1 UE maximum output power for DC 55

6.2B.1.1 Intra-band contiguous EN-DC 55

6.2B.1.2 Intra-band non-contiguous EN-DC 56

6.2B.1.3 Inter-band EN-DC within FR1 56

6.2B.1.3a Inter-band NE-DC within FR1 58

6.2B.1.4 Inter-band EN-DC including FR2 59

6.2B.1.5 Inter-band EN-DC including both FR1 and FR2 59

6.2B.2 UE maximum output power reduction for DC 59

6.2B.2.0 General 59

6.2B.2.1 Intra-band contiguous EN-DC 59

6.2B.2.1.1 General 59

6.2B.2.1.2 MPR for power class 3 and power class 2 60

6.2B.2.2 Intra-band non-contiguous EN-DC 60

6.2B.2.2.1 General 60

6.2B.2.2.2 MPR for power class 3 and power class 2 61

6.2B.2.3 Inter-band EN-DC within FR1 62

6.2B.2.3a Inter-band NE-DC within FR1 62

6.2B.2.4 Inter-band EN-DC including FR2 62

6.2B.2.5 Inter-band EN-DC including both FR1 and FR2 62

6.2B.3 UE additional maximum output power reduction for EN-DC 62

6.2B.3.1 Intra-band contiguous EN-DC 62

6.2B.3.1.0 General 62

6.2B.3.1.1 A-MPR for DC\_(n)71AA 62

6.2B.3.1.2 A-MPR for NS\_04 64

6.2B.3.2 Intra-band non-contiguous EN-DC 66

6.2B.3.2.0 General 66

6.2B.3.2.1 A-MPR for NS\_04 66

6.2B.3.3 Inter-band EN-DC within FR1 68

6.2B.3.3A Inter-band NE-DC within FR1 69

6.2B.3.4 Inter-band EN-DC including FR2 70

6.2B.3.5 Inter-band EN-DC including both FR1 and FR2 70

6.2B.4 Configured output power for DC 70

6.2B.4.1 Configured output power level 70

6.2B.4.1.1 Intra-band contiguous EN-DC 70

6.2B.4.1.2 Intra-band non-contiguous EN-DC 74

6.2B.4.1.3 Inter-band EN-DC within FR1 75

6.2B.4.1.3a Inter-band NE-DC within FR1 78

6.2B.4.1.4 Inter-band EN-DC including FR2 81

6.2B.4.1.5 Inter-band EN-DC including both FR1 and FR2 81

6.2B.4.2 ΔTIB,c for DC 82

6.2B.4.2.0 General 82

6.2B.4.2.1 Intra-band contiguous EN-DC 82

6.2B.4.2.2 Intra-band non-contiguous EN-DC 82

6.2B.4.2.3 Inter-band EN-DC within FR1 82

6.2B.4.2.3.1 ΔTIB,c for EN-DC two bands 82

6.2B.4.2.3.5 ΔTIB,c for EN-DC six bands 95

6.2B.4.2.3a Inter-band NE-DC within FR1 95

6.2B.4.2.4 Inter-band EN-DC including FR2 95

6.2B.4.2.4.1 ΔTIB,c for EN-DC two bands 95

6.2B.4.2.4.2 ΔTIB,c for EN-DC three bands 95

6.2B.4.2.4.3 ΔTIB,c for EN-DC four bands 95

6.2B.4.2.4.4 ΔTIB,c for EN-DC five bands 95

6.2B.4.2.4.5 Void 96

6.2B.4.2.5 Inter-band EN-DC including both FR1 and FR2 96

6.2B.4.2.5.1 ΔTIB,c for EN-DC three bands 96

6.2B.4.2.5.2 ΔTIB,c for EN-DC four bands 96

6.2B.4.2.5.3 ΔTIB,c for EN-DC five bands 96

6.2B.4.2.5.4 ΔTIB,c for EN-DC six bands 96

6.2B.5 Configured output power for NR-DC 96

6.2B.5.1 Configured output power level 96

6.2B.5.1.1 Inter-band NR-DC between FR1 and FR2 96

6.3 Output power dynamics 96

6.3A Output power dynamics for CA 97

6.3B Output power dynamics for DC 97

6.3B.0 General 97

6.3B.1 Output power dynamics for EN-DC with UL sharing from UE perspective 97

6.3B.1.1 E-UTRA and NR switching time mask for TDM based UL sharing from UE perspective 97

6.3B.1a Output power dynamics for NE-DC with UL sharing from UE perspective 98

6.3B.2 Output power dynamics for intra-band EN-DC without dual PA capability 98

6.3B.3 Output power dynamics for intra-band EN-DC with dual PA capability 99

6.4 Void 100

6.4A Transmit signal quality for CA 100

6.4A.1 Frequency error for CA 100

6.4A.2 Transmit modulation quality for CA 100

6.4B Transmit signal quality for DC 100

6.4B.2 Transmit modulation quality for DC 101

6.4B.2.1 Transmit modulation quality for Intra-band contiguous EN-DC 101

6.4B.2.1.1 Error Vector Magnitude 101

6.4B.2.1.2 Carrier leakage 101

6.4B.2.1.3 In-band emissions 101

6.4B.2.2 Transmit modulation quality for Intra-band non-contiguous EN-DC 101

6.4B.2.2.1 Error Vector Magnitude 101

6.4B.2.2.2 Carrier leakage 101

6.4B.2.2.3 In-band emissions 102

6.4B.2.3a Transmit modulation quality for Inter-band NE-DC within FR1 102

6.4B.2.4 Transmit modulation quality for Inter-band EN-DC including FR2 102

6.4B.2.5 Transmit modulation quality for inter-band EN-DC including both FR1 and FR2 102

6.5 Void 102

6.5A Output RF spectrum emissions for CA 102

6.5A.1 Occupied bandwidth for CA 102

6.5A.2 Out-of-band emissions for CA 102

6.5A.3 Spurious emissions for CA 103

6.5A.3.1 Inter-band CA between FR1 and FR2 103

6.5A.4 Transmit intermodulation for CA 103

6.5B Output RF spectrum emissions for DC 103

6.5B.1 Occupied bandwidth for EN-DC 103

6.5B.1.4 Inter-band EN-DC including FR2 103

6.5B.1.5 Inter-band EN-DC including both FR1 and FR2 103

6.5B.2 Out-of-band emissions for DC 103

6.5B.2.1 Intra-band contiguous EN-DC 103

6.5B.2.1.1 Spectrum emissions mask 104

6.5B.2.1.2 Additional spectrum emissions mask 104

6.5B.2.1.2.1 Requirements for network signalled value "NS\_35" 104

6.5B.2.1.2.2 Requirements for network signalled value "NS\_04" 104

6.5B.2.1.3 Adjacent channel leakage ratio 105

6.5B.2.2 Intra-band non-contiguous EN-DC 105

6.5B.2.2.1 Spectrum emissions mask 105

6.5B.2.2.2 Additional spectrum emissions mask 105

6.5B.2.2.3 Adjacent channel leakage ratio 105

6.5B.2.3 Inter-band EN-DC within FR1 106

6.5B.2.3a Inter-band NE-DC within FR1 106

6.5B.2.4 Inter-band EN-DC including FR2 106

6.5B.2.5 Inter-band EN-DC including both FR1 and FR2 106

6.5B.3 Spurious emissions for DC 106

6.5B.3.1 Intra-band contiguous EN-DC 106

6.5B.3.1.1 General spurious emissions 106

6.5B.3.1.2 Spurious emission band UE co-existence 106

6.5B.3.2 Intra-band non-contiguous EN-DC 107

6.5B.3.2.1 General spurious emissions 107

6.5B.3.2.2 Spurious emission band UE co-existence 107

6.5B.3.3 Inter-band EN-DC within FR1 108

6.5B.3.3.2 Spurious emission band UE co-existence 108

6.5B.3.3a Inter-band NE-DC within FR1 117

6.5B.3.3a.1 General spurious emissions 117

6.5B.3.3a.2 Spurious emission band UE co-existence 117

6.5B.3.4 Inter-band EN-DC including FR2 117

6.5B.3.4.1 Spurious emission band UE co-existence 117

6.5B.3.5 Inter-band EN-DC including both FR1 and FR2 117

6.5B.3.5.1 Spurious emission band UE co-existence 117

6.5B.4 Additional spurious emissions 118

6.5B.4.1 General 118

6.5B.4.1.1 Void 118

6.5B.4.2 Intra-band contiguous EN-DC 118

6.5B.4.2.1 Minimum requirement (network signalled value "NS\_04") 118

6.5B.4.3 Intra-band non-contiguous EN-DC 118

6.5B.4.3.1 Minimum requirement (network signalled value "NS\_04") 118

6.5B.4.4 Inter-band EN-DC within FR1 119

6.5B.4.4a Inter-band NE-DC within FR1 119

6.5B.4.5 Inter-band EN-DC including FR2 119

6.5B.4.6 Inter-band EN-DC including both FR1 and FR2 119

6.5B.5 Transmit intermodulation for DC 119

6.5B.5.1 Intra-band contiguous EN-DC 119

6.5B.5.2 Intra-band non-contiguous EN-DC 119

6.5B.5.3 Inter-band EN-DC within FR1 119

6.5B.5.3a Inter-band NE-DC within FR1 119

6.5B.5.4 Inter-band EN-DC including FR2 119

6.5B.5.5 Inter-band EN-DC including both FR1 and FR2 119

6.6B Beam correspondence for DC 120

6.6B.1 Void 120

6.6B.2 Void 120

6.6B.3 Void 120

6.6B.4 Inter-band EN-DC including FR2 120

6.6B.5 Inter-band EN-DC including both FR1 and FR2 120

7 Receiver characteristics 120

7.1 General 120

7.2 Void 121

7.3 Void 121

7.3A Reference sensitivity for CA 121

7.3A.1 General 121

7.3A.2 Reference sensitivity power level for CA 121

7.3A.3 ΔRIB,c for CA 121

7.3A.3.1 ΔRIB,c for Inter-band CA between FR1 and FR2 122

7.3A.4 Void 122

7.3B Reference sensitivity level for DC 122

7.3B.1 General 122

7.3B.2 Reference sensitivity for DC 122

7.3B.2.1 Intra-band contiguous EN-DC 122

7.3B.2.2 Intra-band non-contiguous EN-DC 123

7.3B.2.3 Inter-band EN-DC within FR1 123

7.3B.2.3.1 Reference sensitivity exceptions due to UL harmonic interference for EN-DC in NR FR1 123

7.3B.2.3.2 Reference sensitivity exceptions due to receiver harmonic mixing for EN-DC in NR FR1 127

7.3B.2.3.3 Void 129

7.3B.2.3.4 Reference sensitivity exceptions due to cross band isolation for EN-DC in NR FR1 129

7.3B.2.3.5 MSD for intermodulation interference due to dual uplink operation for EN-DC in NR FR1 131

7.3B.2.3.5.1 MSD test points for intermodulation interference due to dual uplink operation for EN-DC in NR FR1 involving two bands 132

7.3B.2.3.5.2 MSD test points for intermodulation interference due to dual uplink operation for EN-DC in NR FR1 involving three bands 134

7.3B.2.3.5.3 Void 140

7.3B.2.3.6 Reference sensitivity exceptions due to Tx non-linearity interference in 1st or 2nd adjacent channel of UL band for EN-DC in NR FR1 140

7.3B.2.3a Inter-band NE-DC within FR1 141

7.3B.2.3a.1 Reference sensitivity exceptions due to UL harmonic interference for NE-DC in NR FR1 141

7.3B.2.4 Inter-band EN-DC including FR2 141

7.3B.2.4.1 Void 141

7.3B.2.5 Inter-band EN-DC including both FR1 and FR2 141

7.3B.2.5.1 Reference sensitivity exceptions due to UL harmonic interference for EN-DC including both FR1 and FR2 141

7.3B.3 ΔRIB,c, ΔRIBNC for DC 141

7.3B.3.0 General 141

7.3B.3.1 Intra-band contiguous EN-DC 143

7.3B.3.2 Intra-band non-contiguous EN-DC 143

7.3B.3.3 Inter-band EN-DC within FR1 144

7.3B.3.3.1 ΔRIB,c for EN-DC in two bands 144

7.3B.3.3.2 ΔRIB,c for EN-DC three bands 146

7.3B.3.3.4 ΔRIB,c for EN-DC five bands 153

7.3B.3.3.5 ΔRIB,c for EN-DC six bands 155

7.3B.3.3a Inter-band NE-DC within FR1 155

7.3B.3.4 Inter-band EN-DC including FR2 155

7.3B.3.4.1 ΔRIB,c for EN-DC in two bands 155

7.3B.3.4.2 ΔRIB,c for EN-DC three bands 155

7.3B.3.4.3 ΔRIB,c for EN-DC four bands 156

7.3B.3.4.4 ΔRIB,c for EN-DC five bands 156

7.3B.3.4.5 Void 156

7.3B.3.5 Inter-band EN-DC including both FR1 and FR2 156

7.3B.3.5.2 ΔRIB,c for EN-DC three bands 156

7.3B.3.5.3 ΔRIB,c for EN-DC four bands 156

7.3B.3.5.4 ΔRIB,c for EN-DC five bands 156

7.3B.3.5.5 ΔRIB,c for EN-DC six bands 156

7.4 Void 156

7.4A Maximum input level for CA 156

7.4B Maximum input level for DC in FR1 157

7.4B.1 Intra-band contiguous EN-DC in FR1 157

7.4B.2 Intra-band non-contiguous EN-DC in FR1 157

7.4B.3 Inter-band EN-DC within FR1 157

7.5 Void 157

7.5A Adjacent channel selectivity for CA 157

7.5B Adjacent channel selectivity for DC in FR1 158

7.5B.1 Intra-band contiguous EN-DC in FR1 158

7.5B.2 Intra-band non-contiguous EN-DC in FR1 158

7.5B.3 Inter-band EN-DC within FR1 158

7.6 Void 160

7.6A Blocking characteristics for CA 160

7.6B Blocking characteristics for DC in FR1 160

7.6B.1 General 160

7.6B.2 In‑band blocking for DC in FR1 160

7.6B.2.1 Intra-band contiguous EN-DC in FR1 160

7.6B.2.2 Intra-band non-contiguous EN-DC in FR1 160

7.6B.2.3 Inter-band EN-DC within FR1 160

7.6B.3 Out-of-band blocking for DC in FR1 161

7.6B.3.1 Intra-band contiguous EN-DC in FR1 161

7.6B.3.2 Intra-band non-contiguous EN-DC in FR1 161

7.6B.3.3 Inter-band EN-DC within FR1 161

7.6B.3.3a Inter-band NE-DC within FR1 162

7.6B.3.4 Inter-band EN-DC including FR2 163

7.6B.3.5 Inter-band EN-DC including both FR1 and FR2 163

7.6B.4 Narrow band blocking for DC in FR1 163

7.6B.4.1 Intra-band contiguous EN-DC in FR1 163

7.6B.4.2 Intra-band non-contiguous EN-DC in FR1 163

7.6B.4.3 Inter-band EN-DC within FR1 163

7.7 Void 164

7.7A Spurious response for CA 164

7.7B Spurious response for DC in FR1 164

7.7B.1 Intra-band contiguous EN-DC in FR1 164

7.7B.2 Intra-band non-contiguous EN-DC in FR1 164

7.7B.3 Inter-band EN-DC within FR1 164

7.8 Void 165

7.8A Intermodulation characteristics for CA 165

7.8B Intermodulation characteristics for DC in FR1 165

7.8B.1 General 165

7.8B.2 Wide band Intermodulation 165

7.8B.2.1 Intra-band contiguous EN-DC in FR1 165

7.8B.2.2 Intra-band non-contiguous EN-DC in FR1 165

7.8B.2.3 Inter-band EN-DC within FR1 166

7.9 Void 166

7.9A Spurious emissions for CA 166

7.9B Spurious emissions for DC in FR1 166

7.9B.1 Intra-band contiguous EN-DC in FR1 166

7.9B.2 Intra-band non-contiguous EN-DC in FR1 166

7.9B.3 Inter-band EN-DC within FR1 166

Annex A (normative): Measurement channels 167

A.1 General 167

A.2 UL reference measurement channels for E-UTRA TDD Config 2 167

A.2.1 General 167

A.2.2 Reference measurement channels for E-UTRA 168

A.2.2.1 Full RB allocation 168

A.2.2.1.1 QPSK 168

A.2.2.1.2 16-QAM 169

A.2.2.1.3 64-QAM 170

A.2.2.1.4 256 QAM 171

A.2.2.2 Partial RB allocation 172

A.2.2.2.1 QPSK 172

A.2.2.2.2 16-QAM 173

A.2.2.2.3 64-QAM 174

A.2.2.2.4 256 QAM 175

A.3 DL reference measurement channels for E-UTRA 175

A.3.1 General 175

A.3.1.1 QPSK 176

A.3.1.2 64-QAM 177

A.3.1.3 256-QAM 178

Annex B: Void 178

Annex C: Void 178

Annex D: Void 178

Annex E: Void 179

Annex F: Void 179

Annex G: Void 179

Annex H (normative): Modified MPR behavior 179

Annex I (normative): Dual uplink interferer 179

Annex J: Void 180

Annex K: Void 180

Annex L (informative): Change history 181