**3GPP TSG-CT WG1 Meeting #127-eC1-20XXXX**

**Electronic meeting, 13-20 November 2020**

|  |
| --- |
| *CR-Form-v12.0* |
| **CHANGE REQUEST** |
|  |
|  | **24.501** | **CR** | **2845** | **rev** | **1** | **Current version:** | **17.0.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Correction on the condition of filling allowed NSSAI in registration accept message |
|  |  |
| ***Source to WG:*** | ZTE |
| ***Source to TSG:*** | C1 |
|  |  |
| ***Work item code:*** |  5GProtoc17 |  | ***Date:*** | 2020-11-17 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)**Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)* |
|  |  |
| ***Reason for change:*** | The condition of filling allowed NSSAI in registration accept message is incorrect.*b) if:**1) the requested NSSAI was not included in the REGISTRATION REQUEST message or none of the requested NSSAI are allowed;* *2) the network not supporting NSSAA has one or more subscribed S-NSSAIs marked as default that are available; or**3) the network has one or more subscribed S-NSSAIs marked as default which are not subject to network slice-specific authentication and authorization that are available.*The condition should be 1) and 2) or 1) and 3).  |
|  |  |
| ***Summary of change:*** | Correct the condition of filling allowed NSSAI in registration accept message. |
|  |  |
| ***Consequences if not approved:*** | The condition of filling allowed NSSAI in registration accept message is incorrect. |
|  |  |
| ***Clauses affected:*** | 8.2.7.5 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

\*\*\*\*\* First change \*\*\*\*\*

#### 8.2.7.5 Allowed NSSAI

This IE shall be included:

a) if:

1) one or more S-NSSAIs in the requested NSSAI of the REGISTRATION REQUEST message are allowed by the AMF for a network not supporting NSSAA;

2) one or more S-NSSAIs in the requested NSSAI of the REGISTRATION REQUEST message are not subject to network slice-specific authentication and authorization and are allowed by the AMF; or

3) the network slice-specific authentication and authorization has been successfully performed for one or more S-NSSAIs in the requested NSSAI of the REGISTRATION REQUEST message; or

b) if:

1) the requested NSSAI was not included in the REGISTRATION REQUEST message or none of the requested NSSAI are allowed; and

ii) the network not supporting NSSAA has one or more subscribed S-NSSAIs marked as default that are available; or

iii) the network has one or more subscribed S-NSSAIs marked as default which are not subject to network slice-specific authentication and authorization that are available.

\*\*\*\*\* End of change \*\*\*\*\*