**3GPP TSG-CT WG3 Meeting #131C3-235202**

**Chicago, USA, 13 - 17 November, 2023 (revision of C3-235abc)**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.2* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **29.574** | **CR** | **0080** | **rev** | **-** | **Current version:** | **18.3.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Updating the obsoleted IETF HTTP RFC | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Huawei | | | | | | | | | |
| ***Source to TSG:*** | CT3 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | SBIProtoc18 | | | | |  | ***Date:*** | | | 2023-10-25 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **B** |  | | | | | ***Release:*** | | | Rel-18 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | As per the discussion paper in C4-233140 and the agreed CR C4-233140 to TS 29.500 in CT4, in addition to the received LS from CT4 on the same topic in C3-234018, the obsoleted IETF HTTP RFCs need to be updated in this specification. And, replace the terms "payload" and "payload body" with the term "content" in the HTTP messages. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | RFC 7540 replaced by RFC 9113. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Obsolete IEFT HTTP RFCs remain referenced and used in this specification. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 2, 5.1.2.1, 5.2.2.1 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | | This CR does not impact the OpenAPI file. | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

**Additional discussion(if needed):**

**Proposed changes:**

\*\*\* 1st Change \*\*\*

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications".

[2] 3GPP TS 23.501: "System Architecture for the 5G System; Stage 2".

[3] 3GPP TS 23.502: "Procedures for the 5G System; Stage 2".

[4] 3GPP TS 29.500: "5G System; Technical Realization of Service Based Architecture; Stage 3".

[5] 3GPP TS 29.501: "5G System; Principles and Guidelines for Services Definition; Stage 3".

[6] OpenAPI: "OpenAPI Specification Version 3.0.0", <https://spec.openapis.org/oas/v3.0.0>.

[7] 3GPP TR 21.900: "Technical Specification Group working methods".

[8] 3GPP TS 33.501: "Security architecture and procedures for 5G system".

[9] IETF RFC 6749: "The OAuth 2.0 Authorization Framework".

[10] 3GPP TS 29.510: "5G System; Network Function Repository Services; Stage 3".

[11] IETF RFC 9113: "HTTP/2".

[12] IETF RFC 8259: "The JavaScript Object Notation (JSON) Data Interchange Format".

[13] IETF RFC 7807: "Problem Details for HTTP APIs".

[14] 3GPP TS 23.288: "Architecture enhancements for 5G System (5GS) to support network data analytics services".

[15] 3GPP TS 29.520: "5G System; Network Data Analytics Services; Stage 3".

[16] Void.

[17] 3GPP TS 29.571: "5G System; Common Data Types for Service Based Interfaces; Stage 3".

[18] Void.

[19] Void.

[20] Void.

[21] Void.

[22] Void.

[23] 3GPP TS 29.122: "T8 reference point for Northbound APIs".

[24] IETF RFC 6901: "JavaScript Object Notation (JSON) Pointer".

[25] 3GPP TS 29.575: "5G System; Analytics Data Repository Services; Stage 3".

[26] 3GPP TS 29.576: "5G System; Messaging Framework Adaptor Services; Stage 3".

[27] 3GPP TS 29.536: "5G System; Network Slice Admission Control Services; Stage 3".

[28] 3GPP TS 29.554: "5G System; Background Data Transfer Policy Control Service; Stage 3".

[29] 3GPP TS 29.515: "5G System; Gateway Mobile Location Services; Stage 3".

[30] 3GPP TS 29.564: "5G System; User Plane Function Services; Stage 3".

\*\*\* Next Change \*\*\*

#### 5.1.2.1 General

HTTP/2, IETF RFC 9113 [11], shall be used as specified in clause 5 of 3GPP TS 29.500 [4].

HTTP/2 shall be transported as specified in clause 5.3 of 3GPP TS 29.500 [4].

The OpenAPI [6] specification of HTTP messages and content bodies for the Ndccf\_DataManagement API is contained in Annex A.

\*\*\* Next Change \*\*\*

#### 5.2.2.1 General

HTTP/2, IETF RFC 9113 [11], shall be used as specified in clause 5 of 3GPP TS 29.500 [4].

HTTP/2 shall be transported as specified in clause 5.3 of 3GPP TS 29.500 [4].

The OpenAPI [6] specification of HTTP messages and content bodies for the Ndccf\_ContextManagement API is contained in Annex A.

\*\*\* End of Changes \*\*\*