**3GPP TSG-CT WG4 Meeting #99e**

**E-Meeting, 18th – 28th Aug 2020**

|  |
| --- |
| *CR-Form-v12.0* |
| **CHANGE REQUEST** |
|  |
|  | **29.515** | **CR** | **0012** | **rev** | **1** | **Current version:** | **16.1.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | API name correction |
|  |  |
| ***Source to WG:*** | Nokia, Nokia Shanghai Bell |
| ***Source to TSG:*** | CT4 |
|  |  |
| ***Work item code:*** | 5G\_eLCS |  | ***Date:*** | 29-07-2020 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-16 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)**Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)* |
|  |  |
| ***Reason for change:*** | The Service API name is mentioned incorrectly in clause 6.1 of TS 29.515. This CR corrects the API name from “Mgmlc\_Location” to “Ngmlc\_Location”.6 API Definitions6.1 Mgmlc\_Location Service API6.1.1 IntroductionThe Ngmlc\_Location service shall use the Ngmlc\_Location API.The API URI of the Ngmlc\_Location API shall be:**{apiRoot}/<apiName>/<apiVersion>/**The request URIs used in HTTP requests from the NF service consumer towards the NF service producer shall have the Resource URI structure defined in clause 4.4.1 of 3GPP TS 29.501 [6], i.e.:**{apiRoot}/<apiName>/<apiVersion>/<apiSpecificResourceUriPart>**with the following components:- The {apiRoot} shall be set as described in 3GPP TS 29.501 [6].- The <apiName>shall be "ngmlc-loc".- The <apiVersion> shall be "v1".- The <apiSpecificResourceUriPart> shall be set as described in clause 6.1.3. |
|  |  |
| ***Summary of change:*** | Change the API name from “Mgmlc\_Location” to “Ngmlc\_Location” in clause 6.1 |
|  |  |
| ***Consequences if not approved:*** | Inconsistency in Service API name between TS 23.273 and TS 29.515Possibility of wrong implementation at GMLC due to wrong service API name in TS 29.515 |
|  |  |
| ***Clauses affected:*** | 6.1 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | No impact on openAPI |
|  |  |
| ***This CR's revision history:*** |  |

\* \* \* First Change \* \* \* \*

# 6 API Definitions

## 6.1 Ngmlc\_Location Service API

### 6.1.1 Introduction

The Ngmlc\_Location service shall use the Ngmlc\_Location API.

The API URI of the Ngmlc\_Location API shall be:

**{apiRoot}/<apiName>/<apiVersion>/**

The request URIs used in HTTP requests from the NF service consumer towards the NF service producer shall have the Resource URI structure defined in clause 4.4.1 of 3GPP TS 29.501 [6], i.e.:

**{apiRoot}/<apiName>/<apiVersion>/<apiSpecificResourceUriPart>**

with the following components:

- The {apiRoot} shall be set as described in 3GPP TS 29.501 [6].

- The <apiName>shall be "ngmlc-loc".

- The <apiVersion> shall be "v1".

- The <apiSpecificResourceUriPart> shall be set as described in clause 6.1.3.

\* \* \* End of Changes \* \* \* \*