**3GPP TSG-CT WG4 Meeting #99eC4-204abc**

**E-Meeting, 18th – 28th June 2020 *was* C4-204322**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.0* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **29.515** | **CR** | **0018** | **rev** | **1** | **Current version:** | **16.1.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Corrections on LocationData | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Huawei | | | | | | | | | |
| ***Source to TSG:*** | CT4 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | 5G\_eLCS | | | | |  | ***Date:*** | | | 2020-08-11 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **F** |  | | | | | ***Release:*** | | | Rel-16 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) Rel-12 (Release 12)* *Rel-13 (Release 13) Rel-14 (Release 14) Rel-15 (Release 15) Rel-16 (Release 16)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | AMF may contain the result of notification and verification (see 29.518 clause 6.4.6.2.3) in the response of service operation Retrieve UE Location to GMLC, When UE is roaming and (V)GMLC is used, the result of notification and verification from will be forwarded by (V)GMLC to (H)GMLC,therefore it should be present in operation provide-location response from VGMLC to HGMLC of Ngmlc if available.  Apart from the result of notification and verification, altitude, servingLMFIdentification should be forwarded by (V)GMLC to (H)GMLC if received from AMF when UE is roaming and VGMLC is applied. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | 1. Added reference of 3GPP TS 29.518 in clause 2. 2. Added attribute locationPrivacyVerResult in data model LocationData (used in response body of operation provide-location). 3. Added ecgi, ncgi, barometricPressure, altitude, servingLMFIdentification in data model LocationData | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Current description may lead to different interpretations and implementations which may raise trouble in interoperability between different vendors. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 2, 6.1.5.1, 6.1.5.2.3, A.2 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | | This CR will introduce backward compatible corrections in the OpenAPI specification file of TS29515\_Ngmlc\_Location.yaml. | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | | Rev1:   1. Removded new attributes ecgi, ncgi, barometricPressure from the definition of data model LocationData because they won't be delivered to HPLMN. | | | | | | | | |

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*Information\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications".

[2] 3GPP TS 23.501: "System Architecture for the 5G System; Stage 2".

[3] 3GPP TS 23.502: "Procedures for the 5G System; Stage 2".

[4] 3GPP TS 23.273: "5G System Location Services (LCS)".

[5] 3GPP TS 29.500: "5G System; Technical Realization of Service Based Architecture; Stage 3".

[6] 3GPP TS 29.501: "5G System; Principles and Guidelines for Services Definition; Stage 3".

[7] OpenAPI Initiative, "OpenAPI 3.0.0 Specification", <https://github.com/OAI/OpenAPI-Specification/blob/master/versions/3.0.0.md>.

[8] IETF RFC 7540: "Hypertext Transfer Protocol Version 2 (HTTP/2)".

[9] IETF RFC 8259: "The JavaScript Object Notation (JSON) Data Interchange Format".

[10] IETF RFC 7807: "Problem Details for HTTP APIs".

[11] 3GPP TS 29.571: "5G System; Common Data Types for Service Based Interfaces; Stage 3".

[12] 3GPP TS 29.572: "5G System; Location Management Services; Stage 3".

[13] ITU Recommendation E.164: "The international public telecommunication numbering plan".

[14] 3GPP TS 29.503: "5G System; Unified Data Management Services; Stage 3".

[15] 3GPP TS 33.501: "Security architecture and procedures for 5G system".

[16] IETF RFC 6749: "The OAuth 2.0 Authorization Framework".

[17] 3GPP TS 29.510: "Network Function Repository Services; Stage 3".

[18] 3GPP TS 22.071: "Location Services (LCS); Service description; Stage 1".

[19] 3GPP TR 21.900: "Technical Specification Group working methods".

[xx] 3GPP TS 29.518: "5G System; Access and Mobility Management Services; Stage 3".

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*Next change\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

#### 6.1.5.1 General

This clause specifies the application data model supported by the API.

Table 6.1.5.1-1 specifies the data types defined for the Ngmlc\_Location service based interface protocol.

Table 6.1.5.1-1: Ngmlc\_Location specific Data Types

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | Clause defined | Description | Applicability |
| InputData | 6.1.5.2.2 | the input parameters in ProvideLocation service operation |  |
| LocationData | 6.1.5.2.3 | the response parameters in ProvideLocation service operation |  |
| CancelLocData | 6.1.5.2.4 | the input parameters in CancelLocation service operation |  |
| LocUpdateData | 6.1.5.2.5 | the input parameters in LocationUpdate service operation |  |
| EventNotifyData | 6.1.5.2.6 | the input parameters in EventNotify Notification service operation |  |
| UePrivacyRequirements | 6.1.5.2.7 | UE privacy requirements from (H)GMLC to the serving AMF or VGMLC(in the roaming case) for the target UE |  |
| LocUpdateNotification | 6.1.5.2.9 | Location Update Notification |  |
| ServiceIdentity | 6.1.5.3.2 | service identity |  |
| CodeWord | 6.1.5.3.2 | codeword |  |
| ExternalClientIdentification | 6.1.5.3.2 | external client identification |  |
| E164CountryCodeOfGeographicArea | 6.1.5.3.2 | E.164 country codes for geographic areas |  |
| PseudonymIndicator | 6.1.5.3.3 | It defines if a pseudonym is requested |  |
| LocationRequestType | 6.1.5.3.4 | NI-LR, MT-LR or MO-LR |  |
| LocationTypeRequested | 6.1.5.3.5 | the location type requested by the LCS client |  |
| EventNotifyDataType | 6.1.5.3.6 | the type of event that triggers event notification |  |

Table 6.1.5.1-2 specifies data types re-used by the Ngmlc\_Location service based interface protocol from other specifications, including a reference to their respective specifications and when needed, a short description of their use within the Ngmlc\_Location service based interface.

Table 6.1.5.1-2: Ngmlc\_Location re-used Data Types

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | Reference | Comments | Applicability |
| Gpsi | 3GPP TS 29.571 [11] |  |  |
| Supi | 3GPP TS 29.571 [11] |  |  |
| Uri | 3GPP TS 29.571 [11] |  |  |
| AmfId | 3GPP TS 29.571 [11] |  |  |
| NfInstanceId | 3GPP TS 29.571 [11] |  |  |
| ExternalClientType | 3GPP TS 29.572 [12] |  |  |
| LocationQoS | 3GPP TS 29.572 [12] |  |  |
| LcsQosClass | 3GPP TS 29.572 [12] |  |  |
| SupportedGADShapes | 3GPP TS 29.572 [12] |  |  |
| PeriodicEventInfo | 3GPP TS 29.572 [12] |  |  |
| AreaEventInfo | 3GPP TS 29.572 [12] |  |  |
| MotionEventInfo | 3GPP TS 29.572 [12] |  |  |
| LdrType | 3GPP TS 29.572 [12] |  |  |
| LdrReference | 3GPP TS 29.572 [12] |  |  |
| AgeOfLocationEstimate | 3GPP TS 29.572 [12] |  |  |
| PositioningMethod | 3GPP TS 29.572 [12] |  |  |
| AccuracyFulfilmentIndicator | 3GPP TS 29.572 [12] |  |  |
| LmfIdentification | 3GPP TS 29.572 [12] |  |  |
| LcsServiceType | 3GPP TS 29.572 [12] |  |  |
| VelocityRequested | 3GPP TS 29.572 [12] |  |  |
| LcsPriority | 3GPP TS 29.572 [12] |  |  |
| VelocityEstimate | 3GPP TS 29.572 [12] |  |  |
| TerminationCause | 3GPP TS 29.572 [12] |  |  |
| PositioningMethodAndUsage | 3GPP TS 29.572 [12] |  |  |
| GnssPositioningMethodAndUsage | 3GPP TS 29.572 [12] |  |  |
| LcsServiceAuth | 3GPP TS 29.571 [11] |  |  |
| LocationPrivacyVerResult | 3GPP TS 29.518 [xx] |  |  |

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*Next change\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

##### 6.1.5.2.3 Type: LocationData

Table 6.1.5.2.3-1: Definition of type LocationData

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| gpsi | Gpsi | O | 0..1 | Generic Public Subscription Identitfier |  |
| supi | Supi | O | 0..1 | Subscription Permanent Identifier |  |
| locationEstimate | GeographicArea | O | 0..1 | Geographic area of the target UE |  |
| civicAddress | CivicAddress | O | 0..1 | Civic address of the target UE |  |
| ageOfLocationEstimate | AgeOfLocationEstimate | O | 0..1 | Age of location estimate |  |
| positioningDataList | array(PositioningMethodAndUsage) | O | 1..N | If present, this IE shall indicate the usage of each non-GANSS positioning method that was attempted to determine the location estimate, either successfully or unsuccessfully. |  |
| gnssPositioningDataList | array(GnssPositioningMethodAndUsage) | O | 1..N | If present, this IE shall indicate the usage of each GANSS positioning method that was attempted to determine the location estimate, either successfully or unsuccessfully. |  |
| accuracyFulfilmentIndicator | AccuracyFulfilmentIndicator | O | 0..1 | The indication whether the obtained location estimate satisfies the requested accuracy or not |  |
| ueVelocity | VelocityEstimate | O | 0..1 | Responded UE velocity, if requested and available |  |
| ldrReference | LdrReference | C | 0..1 | Notification correlation ID  It shall be present in the response to NEF if it is allocated by HGMLC for the the Deferred 5GC-MT-LR procedure. |  |
| altitude | Altitude | C | 0..1 | If present, this IE indicates the altitude of the positioning estimate.  This IE shall be sent from (V)GMLC to (H)GMLC if received by VGMLC from AMF when roaming. |  |
| servingLMFIdentification | LMFIdentification | C | 0..1 | If present, this IE contains the identification of a serving LMF for periodic or triggered location.  This IE shall be sent from (V)GMLC to (H)GMLC if received by VGMLC from AMF when roaming. |  |
| locationPrivacyVerResult | LocationPrivacyVerResult | C | 0..1 | If present, this IE contains the result of location privacy verification by UE.  The IE shall be included from (V)GMLC to (H)GMLC if received from the serving AMF by (V)GMLC when roaming and a location request with notification and privacy verification only indication is sent to the serving AMF via (V)GMLC by (H)GMLC during location request procedure.. |  |

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*Next change\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

## A.2 Ngmlc\_Location API

openapi: 3.0.0

***(… text not shown for clarity …)***

LocationData:

type: object

properties:

gpsi:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

supi:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

locationEstimate:

$ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/GeographicArea'

civicAddress:

$ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/CivicAddress'

ageOfLocationEstimate:

$ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/AgeOfLocationEstimate'

positioningDataList:

type: array

items:

$ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/PositioningMethodAndUsage'

minItems: 1

gnssPositioningDataList:

type: array

items:

$ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/GnssPositioningMethodAndUsage'

minItems: 1

accuracyFulfilmentIndicator:

$ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/AccuracyFulfilmentIndicator'

ueVelocity:

$ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/VelocityEstimate'

ldrReference:

$ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/LdrReference'

altitude:

$ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/Altitude'

servingLMFIdentification:

$ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/LMFIdentification'

locationPrivacyVerResult:

$ref: 'TS29518\_Namf\_Location.yaml#/components/schemas/LocationPrivacyVerResult'

***(… text not shown for clarity …)***

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*The end of changes\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*