3GPP TSG-RAN #93-e RP-21xxxx  
Online, 13-17 September 2021

Agenda Item: 9.8, 14

Source: RAN2 Chair (Moderator)

Title: Report of Offline Discussion [93e-29-UECapability]

Document for: Discussion

# Introduction

This discussion includes RP-212108 [1], RP-212109 [2], RP-212206 [3], RP-212207 [4].

# Contacts

Please provide a company contact that the email discussion moderator can contact if required.

|  |  |
| --- | --- |
| **Company** | **Contact name and email** |
| Moderator | Johan.Johansson@mediatek.com |
| Qualcomm | pgaal@qti.qualcomm.com |
| Ericsson | mattias.a.bergstrom@ericsson.com |
| Apple | naveen.palle@apple.com |
| T-Mobile USA | John.humbert2@t-mobile.com |
| Huawei,  HiSilicon | zhaoyang@huawei.com |
| Futurewei | hao.bi@futurewei.com |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

# NR URLLC UE categories/profiles

RP-212109 [2] and RP-212207 [4] (with CR in RP-212206 [3]), discusses NR URLLC UE categories/profiles or improved description of features for NR URLLC.

The topic was discussed also at previous TSG RAN meeting.

Status, TSG RAN 92e:

*There is no consensus at current meeting. Accurate status of discussion:*

*a) There seems to be full agreement that defining URLLC profiles / UE categories will consume a lot of time and is not easy, e.g. it is commented that there are different diverse URLLC applications with different requirements.*

*b) The proponents seems to be in agreement that the purpose of defining URLLC profiles / UE categories is to bring clarity to the market as to which features are relevant for URLLC, and to avoid market fragmentation. Also some companies opposing to do this in 3GPP acknowledges that there would be value to have this.*

*c) It is questioned that 3GPP is not the right place to address issues such as market fragmentation. To do this work, involvement of industry players not in 3GPP may be needed. It is pointed out that in 3GPP it may be particularly difficult to converge as companies are likely to push for their own solutions.*

*d) The need is questioned by some companies. From technical perspective UE capabilities are unambiguous, now also the TR38.822 has been updated for easier navigation.*

*e) A majority of companies think such effort is not worthwhile in 3GPP, while several major operators support this.*

*f) There is some support among proponents to attempt to simplify the work by having limitations, e.g. limiting to Rel-15 only in a first step, and treating features for latency and reliability separately. It is also commented that it would be valuable to define a basic feature set that meets certain requirements in basic scenario, to be used as baseline.*

RP-212109 [2] suggests that mainly c) above need to be further discussed and addressed in addition to more exactly decide what to specify, in order to have NR URLLC UE categories/profiles.

RP-212109 [2] further suggests that in order to make the work feasible, not full NR URLLC UE categories/profiles can be specified, e.g. according to examples below (Alt 1, Alt 2) or other way.

* **(Alt. 1)** Even though so many kind of categories (e.g. reliability only, low latency only, reliability + latency) may be needed to cover the potential URLLC use cases, RAN can focus on defining only one category/profile for now.
* **(Alt. 2)** Do not define any categories/profiles, but introduce new categorization for URLLC related UE features in TS38.822 based on their characteristics to give more detailed technical analyses to outside 3GPP, for example:
  + Features related to achieve 99.9999% reliability:
    - 5-34b, 5-34a …
  + Features related to achieve 1ms latency in radio interface:
    - 5-5a, 5-5b, 5-5c …
  + Features related to capacity enhancement for URLLC
    - Xxx
  + [Other dimensions can be discussed]
  + [Target release (i.e. Rel-15 only or also include Rel-16) needs to be clarified]

RP-212207 [4] (with CR in RP-212206 [3]) Observes that which Rel-15 features are relevant to URLLC type of services is not currently visible externally, as all Rel-15 features are listed together in [TR38.822](https://www.3gpp.org/DynaReport/38822.htm) and suggest to capture the Rel-15 UE capabilities relevant for URLLC operation as an informative annex in TS38.306 (e.g. as illustrated in [RP-212206](https://www.3gpp.org/ftp/tsg_ran/TSG_RAN/TSGR_93e/Docs/RP-212206.zip)) **(Alt. 3)**

## Initial Round

Q: Moderator asks companies to provide initial feedback on the observations and proposals in RP-212109 [2] and RP-212207 [4], e.g. on Alt 1 Alt 2 Alt 3, to what extent they are acceptable, and whether other details need to be considered.

|  |  |  |
| --- | --- | --- |
| **Company** | **Acceptable Alt** | **Comment / Justification / Explanation** |
| Qualcomm | Alt 3 | Alt 1 and Alt 2 are already precluded as per the previous conclusions. None of the alternatives are strictly speaking necessary but we can accept Alt 3 in order to close this issue. |
| Ericsson | - | We believe that the conclusions from the last RAN plenary meeting still hold and that 3GPP is not the fora to define these categories. As discussed earlier, it is better if this type of exercise is handled outside of 3GPP and it is already ongoing in some industry fora, e.g. 5G-ACIA. |
| Apple | No, but see comments. | |  | | --- | | As discussed earlier the existing UE capabilities have been defined in a generic way to support a wide range of requirements for a variety of use-cases, products, and applications. Thus Alt 1 and Alt 2 may end up with many many combinations. At the same time, adding all these variants into a specification may not be so essential.  We still do not think any of the alternatives is necessary. **But if it helps, we can accept Alt 3 with some modification. Our preference would be to use the table proposed by Nokia in Alt 3, but ideally the table would be more suitable to be placed into 38.822** (e.g., section 4), since the TR already provides additional information for other features including a grouping, and this could be extended with a view to URLLC specifically. | |
| T-Mobile USA | - | Trying to define profiles for URLLC will be as unproductive as the FGI bit discussion that RAN had for early releases of LTE and subsequently for Mandatory with Capability bit indication for NR.  Implementors will tailer their solutions to market needs. With the large number of use cases for URLLC we don’t see a need to define profiles or groups of features |
| Huawei,  HiSilicon | Need further discussion  Sort of combined Alt 2 and Alt3 | We are in general positive on figuring out a way forward on defining URLLC UE type/category.  Alt 2 makes sense as URLLC services could differ on different E2E latency and reliability classification, but as several companies pointed out already in RAN#92e, these detailed requirements may need inputs from the industry players. We observed that 5G-ACIA is having relevant activities, and it would be good to coordinate with the industry, to make the URLLC UE type/category definition useful and consistent with the real marketing requirements. Thus we suggest to send an LS to 5G-ACIA, informing that 3GPP is discussing how to define the URLLC UE type/categories, and ask 5G-ACIA to provide necessary inputs to help such definition.  In parallel with coordination with 5G-ACIA, Alt 3 can first be discussed in 3GPP to at least identify those capabilities which are specific to URLLC. It would be better if the capabilities can be grouped into low-latency specific and reliability specific. This may help future discussion once the latency and reliability requirements classification becomes clearer. |
| Samsung | Alt. 3 | We think that alt. 1 is to define basic feature group for URLLC and alt. 2 is to define details of URLLC categories for all UE capability. These are already discussed in last meeting and any consensus wasn’t achieved. With minimum 3GPP efforts, we can accept alt. 3. |
| Futurewei | - | We are also concerned that more exercises to specify URLLC profiles/categories in RAN without industry input may not be very productive, and we would be open to work on this issue jointly with industrial fora.  If there happens to be agreement to capture something for URLLC feature, we’d prefer Alt. 2 to keep it consistent with other efforts of updating UE features. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

# UL MIMO coherence capabilities

RP-212108 [1] proposes to address LS from RAN4 to RAN1 and RAN2 in R4-2107765 (R1-2106431) due to lack of progress in WGs. Moderator observes that in RAN2 the topic was postponed awaiting outcome from RAN1. The following proposals are made:

Proposal 1: A new UE capability indicating UL MIMO coherence per band per band combination is introduced (regardless of UL Tx switching)

Proposal 2: Solve this issue at the RAN#93-emeeting.

## Initial Round

Q: Moderator asks companies to provide initial feedback on the proposals and discussion in RP-212108 [1], i.e. whether to have the discussion at TSG RAN 93e, and/or whether the proposed technical way forward or other way forward can be acceptable.

|  |  |  |
| --- | --- | --- |
| **Company** | **Acceptable?** | **Comment / Justification / Explanation** |
| Qualcomm | Yes | We support discussing and solving this issue in RAN#93e.  The UE MIMO coherence capability is strongly coupled with the number of Tx chains / layers. For example, the UE may be coherent capable with 2 Tx but not coherent (not even partial coherent) with 4 Tx. Since the number of layers is already signaled per band per band combination, the coherence capability needs to be signaled in the same structure per band per band combination to maintain consistency and avoid under reporting by the UE. |
| Ericsson | No | The UL TX switching issue for coherent MIMO operation that was identified in the RAN4 LS R1-2106431 is already solved in our view by the CR made to 38.101, and it so does not drive the need for the UE capability changes suggested in RP-212108. |
| Apple | Yes, but | We are ok to introduce a per-band-per-BC capability, but regarding the topic getting this discussed/resolved in RAN-93e, we are not sure if this is needed. Can be done at WG level. |
| Huawei,  HiSilicon | No | We had similar views as Ericsson. |
| Samsung | No | We also think gNB can manage this issue based on R4-2109583 for 38.101 but we think this discussion can be done in WG discussion. |
| Futurewei |  | This should be resolved at WG level. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

# Other Rounds

Etc.

# References

[1] RP-212108 UL MIMO coherence capabilities Qualcomm Incorporated   
 Discussion

[2] RP-212109 NR UE categories/profiles for URLLC SoftBank Discussion

[3] RP-212206 Introduction of informative annex on list of Rel-15 features relevant to   
 URLLC Nokia, Nokia Shanghai Bell CR Rel-16 38.306  
 16.5.0 0644 - F NR\_newRAT-Core

[4] RP-212207 Discussion on introduction of list of Rel-15 features relevant to URLLC   
 Nokia, Nokia Shanghai Bell Discussion